{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Price List 2019-2020","Sheet1"],"not_rendered":{"charts":0,"images":4,"macros":1,"external_links":0,"defined_names":3,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Price List 2019-2020","index":0,"n_rows":158880,"n_cols":9,"rows_kept":4500,"cut":true,"hidden":false,"merged":[[0,1,0,2],[0,3,0,7],[1,0,1,7],[2,2,2,7],[2,0,2,1]],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
[null,"Siemens Digital Industries\nΤιμοκατάλογος Προϊόντων Βιομηχανίας 2019-2020",null,"Ισχύει από την 01.10.2019 και καταργεί κάθε προηγούμενο. Οι τιμές και τα τεχνικά χαρακτηριστικά των υλικών υπόκεινται σε οποιαδήποτε αλλαγή χωρίς προηγούμενη ειδοποίηση και δεν περιλαμβάνουν ΦΠΑ. "]
["Περιλαμβάνει τις παρακάτω κατηγορίες υλικών:"]
["Βιομηχανικός αυτοματισμός Simatic και Υλικά Δικτύου (Simatic)\nΒιομηχανικός αυτοματισμός Simatic S71200 (S71200)\nLOGO!, τροφοδοτικά LOGO! Power (LOGO!)\nΚινητήρες AC (LVM) \n",null,"Διανομή ισχύος χαμηλής τάσης και Τεχνολογία ηλεκτρικών εγκαταστάσεων (LP) \nΡυθμιστές στροφών και συστήματα ελέγχου κίνησης  Motion control (MC)\nΒιομηχανικό υλικό χαμηλής τάσης (CP)"]
["Αναζήτηση υλικού","Αναζήτηση με:"]
["Κωδικός","Περιγραφή","Τιμή καταλόγου (€)","Μον. Μέτρησης","Ποσ. μονάδας μέτρησης","Κατηγορία υλικού","Βάρος (KG)","Ελάχιστη ποσότητα παραγγελίας"]
["6AG1000-5CL01-4FA0","SIPLUS Conti Bundle 427E B2 0β€¦+55Β°C With Conformal Coating based on 6BK1000-5CL01-1FA0 . - SIPLUS IPC427E, - SIMATIC IPC DiagMonitor, - SIMATIC S7-1500 Failsafe SW Controller CPU 1507S F, - SIMATIC OPC UA S7-1500 Medium Single Runtime License",4531,"ST",1,"SIMATIC",3.2650000000000001,1,"6AG10005CL014FA0"]
["6AG1000-5CL01-4FB0","SIPLUS Conti Bundle 427E B6 0β€¦+55 Β°C With conformal coating based on 6BK1000-5CL01-1FB0 . - SIPLUS IPC427E, - SIMATIC IPC DiagMonitor, - SIMATIC S7-1500 Failsafe SW Controller CPU 1507S F, - SIMATIC WinCC Runtime Advanced 512 PowerTags - SIMATIC WinCC Recipes+Logging for Runtime Advanced - SIMATIC OPC UA S7-1500 Medium Single Runtime License",5550,"ST",1,"SIMATIC",3.2650000000000001,1,"6AG10005CL014FB0"]
["6AG1000-5CL01-4FB1","SIPLUS Conti Bundle 427E B7 0β€¦+55Β°C with Conformal Coating based on 6BK1000-5CL01-1FB1 . - SIPLUS IPC427E, - SIMATIC IPC DiagMonitor, - SIMATIC S7-1500 Failsafe SW Controller CPU 1507S F, - SIMATIC WinCC Runtime Advanced 2048 PowerTags, - SIMATIC WinCC Recipes + Logging for Runtime Advanced, - SIMATIC OPC UA S7-1500 Medium Single Runtime License",6232,"ST",1,"SIMATIC",3.2650000000000001,1,"6AG10005CL014FB1"]
["6AG1000-5CL01-4FB2","SIPLUS Conti Bundle 427E B6 0β€¦+55 Β°C With conformal coating based on 6BK1000-5CL01-1FB2 . - SIPLUS IPC427E, - SIMATIC IPC DiagMonitor, - SIMATIC S7-1500 Failsafe SW Controller CPU 1507S F, - SIMATIC WinCC Runtime Advanced 4096 PowerTags - SIMATIC WinCC Recipes+Logging for Runtime Advanced - SIMATIC OPC UA S7-1500 Medium Single Runtime License",7121,"ST",1,"SIMATIC",3.2650000000000001,1,"6AG10005CL014FB2"]
["6AG1000-5CL01-4XA0","SIPLUS Conti Bundle 427E B1 0β€¦+55Β°C with Conformal Coating based on 6BK1000-5CL01-1XA0 . - SIPLUS IPC427E, - SIMATIC IPC DiagMonitor, - SIMATIC S7-1500 SW Controller CPU 1507S, - SIMATIC OPC UA S7-1500 Medium Single Runtime License",4206,"ST",1,"SIMATIC",3.2650000000000001,1,"6AG10005CL014XA0"]
["6AG1000-5CL01-4XB0","SIPLUS Conti Bundle 427E B3 0β€¦+55 Β°C With conformal coating based on 6BK1000-5CL01-1XB0 . - SIPLUS IPC427E, - SIMATIC IPC DiagMonitor, - SIMATIC S7-1500 SW Controller CPU 1507S, - SIMATIC WinCC Runtime Advanced 512 PowerTags - SIMATIC WinCC Recipes+Logging for Runtime Advanced - SIMATIC OPC UA S7-1500 Medium Single Runtime License",5164,"ST",1,"SIMATIC",3.2650000000000001,1,"6AG10005CL014XB0"]
["6AG1000-5CL01-4XB1","SIPLUS Conti Bundle 427E B4 0β€¦+55 Β°C With conformal coating based on 6BK1000-5CL01-1XB1 . - SIPLUS IPC427E, - SIMATIC IPC DiagMonitor, - SIMATIC S7-1500 SW Controller CPU 1507S, - SIMATIC WinCC Runtime Advanced 2048 PowerTags - SIMATIC WinCC Recipes+Logging for Runtime Advanced - SIMATIC OPC UA S7-1500 Medium Single Runtime License",5827,"ST",1,"SIMATIC",3.2650000000000001,1,"6AG10005CL014XB1"]
["6AG1000-5CL01-4XB2","SIPLUS Conti Bundle 427E B5 0β€¦+55 Β°C With conformal coating based on 6BK1000-5CL01-1XB2 . - SIPLUS IPC427E, - SIMATIC IPC DiagMonitor, - SIMATIC S7-1500 SW Controller CPU 1507S, - SIMATIC WinCC Runtime Advanced 4096 PowerTags - SIMATIC WinCC Recipes+Logging for Runtime Advanced - SIMATIC OPC UA S7-1500 Medium Single Runtime License",6787,"ST",1,"SIMATIC",3.2650000000000001,1,"6AG10005CL014XB2"]
["6AG1010-1AU00-4AA0","SIPLUS SIMOCODE pro V Basic unit 2 -25...+60Β°C with conformal coating based on 3UF7010-1AU00-0 . E- type with \"Safety \"\"12 Mbit/s, RS485;\"\"\" \"4I/3O freely parameterizable;\" \"US: 110-240V AC/DC; input for\" \"thermistor connection;\" \"monostable relay outputs;\" expandable by extension modules",672,"ST",1,"SIMATIC",0.35,1,"6AG10101AU004AA0"]
["6AG1040-1LA00-2AA0","SIPLUS S120 Control Unit CU310-2 DP -20...+55Β°C with conformal coating based on 6SL3040-1LA00-0AA0 . with PROFIBUS interface without CompactFlash card",1197,"ST",1,"SIMATIC",0.79,1,"6AG10401LA002AA0"]
["6AG1040-1LA01-2AA0","SIPLUS S120 Control Unit CU310-2 PN -20...+55Β°C with conformal coating based on 6SL3040-1LA01-0AA0 . with PROFINET interface without CompactFlash card",1197,"ST",1,"SIMATIC",0.95,1,"6AG10401LA012AA0"]
["6AG1052-1CC08-7BA0","SIPLUS LOGO! 24CE -20...+70Β°C start up -20Β°C with conformal coating based on 6ED1052-1CC08-0BA0 . logic module, Display PS/I/O: 24 V/24 V/24 V trans., 8 DI (4AI)/4DO, memory 400 blocks, modular expandable, Ethernet integr. web server, data log, user-defined Web pages, standard microSD card for LOGO! Soft Comfort V8 or higher, older projects executable",328,"ST",1,"LOGO!",0.25,1,"6AG10521CC087BA0"]
["6AG1052-1FB08-7BA0","SIPLUS LOGO! 230RCE -20 ... +70Β°C start up -20Β°C with conformal coating based on 6ED1052-1FB08-0BA0 . logic module, display PS/I/O: 115V/230V/relay, 8 DI/4 DO, memory 400 blocks, modular expandable, Ethernet, integr. web server, data log, user-defined Web pages, standard microSD card for LOGO! Soft Comfort V8 or higher, older projects executable",350,"ST",1,"LOGO!",0.25,1,"6AG10521FB087BA0"]
["6AG1052-1HB08-7BA0","SIPLUS LOGO! 24RCE -20 ...+70Β°C start up -20Β°C with conformal coating based on 6ED1052-1HB08-0BA0 . logic module,Display PS/I/O: 24 V AC/24 V DC/relay, 8 DI/4 DO, memory 400 blocks, modular expandable, Ethernet, integr. web server, data log, user- defined Web pages, standard microSD card for LOGO! Soft Comfort V8 or higher, older projects executable",346,"ST",1,"LOGO!",0.3,1,"6AG10521HB087BA0"]
["6AG1052-1MD08-7BA0","SIPLUS LOGO! 12/24RCE -20 ... +70Β°C start up -20Β°C with conformal coating based on 6ED1052-1MD08-0BA0 . Logikmodul, Display SV/E/A: 24V/24V/24V trans., 8DE (4AE)/4DA, SP. 400 blocks, modular erweiterbar, Ethernet integr. Web-Server, Datalog, benutzerdefinierte Web-Seiten, Standard microSD-Karte fΓΌr LOGO! Soft Comfort ab V8, Γ¤ltere Projekte ablauffΓ¤hig",375,"ST",1,"LOGO!",0.3,1,"6AG10521MD087BA0"]
["6AG1052-2CC08-7BA0","SIPLUS LOGO! 24CEO -40...+70Β°C start up -25Β°C with conformal coating based on 6ED1052-2CC08-0BA0 . logic module, without display, PS/I/O: 24 V/24 V/24 V trans., 8 DI (4AO)/4DO, memory 400 blocks, modularly expandable, Ethernet, integr. web server, data log, user-defined web pages, standard microSD card for LOGO! SOFT Comfort V8 or higher, older projects can be run",298,"ST",1,"LOGO!",0.22500000000000001,1,"6AG10522CC087BA0"]
["6AG1052-2FB08-7BA0","SIPLUS LOGO! 230RCEO -40...+70Β°C start up -25Β°C mit conformal coating based on 6ED1052-2FB08-0BA0 . Logikmodul, Display SV/E/A: 24V/24V/24V trans., 8DE (4AE)/4DA, SP. 400 blocks, modular erweiterbar, Ethernet integr. Web-Server, Datalog, benutzerdefinierte Web-Seiten, Standard microSD-Karte fΓΌr LOGO! Soft Comfort ab V8, Γ¤ltere Projekte ablauffΓ¤hig",304,"ST",1,"LOGO!",0.25,1,"6AG10522FB087BA0"]
["6AG1052-2HB08-7BA0","SIPLUS LOGO! 24RCEO (AC) -40...+70Β°C start up -25Β°C with conformal coating based on 6ED1052-2HB00-0BA8 . Logikmodul, Display SV/E/A: 24V/24V/24V trans., 8DE (4AE)/4DA, SP. 400 blocks, modular erweiterbar, Ethernet integr. Web-Server, Datalog, benutzerdefinierte Web-Seiten, Standard microSD-Karte fΓΌr LOGO! Soft Comfort ab V8, Γ¤ltere Projekte ablauffΓ¤hig",294,"ST",1,"LOGO!",0.25,1,"6AG10522HB087BA0"]
["6AG1052-2MD08-7BA0","SIPLUS LOGO! 12/24RCEO -40...+70Β°C start up -25Β°C mit conformal coating based on 6ED1052-2MD08-0BA0 . Logikmodul, Display SV/E/A: 24V/24V/24V trans., 8DE (4AE)/4DA, SP. 400 blocks, modular erweiterbar, Ethernet integr. Web-Server, Datalog, benutzerdefinierte Web-Seiten, Standard microSD-Karte fΓΌr LOGO! Soft Comfort ab V8, Γ¤ltere Projekte ablauffΓ¤hig",330,"ST",1,"LOGO!",0.25,1,"6AG10522MD087BA0"]
["6AG1055-0AA00-2BA0","SIPLUS S120 BOP20 Basic Operator Panel -20...+70Β°C with conformal coating based on 6SL3055-0AA00-4BA0 . Actuator with miniature display 2-line, 6 keys for parameter assignment and diagnostics suitable for Control Units CU305, CU310, CU320",143,"ST",1,"SIMATIC",5.3999999999999999E-2,1,"6AG10550AA002BA0"]
["6AG1055-1CB00-7BA2","SIPLUS LOGO! DM8 24 -40...+70 Β°C start up -25Β°C with conformal coating based on 6ED1055-1CB00-0BA2 . Expansion module, PS/I/O: 24V/24V/trans., 4 DI/4 DO for LOGO! 8",182,"ST",1,"LOGO!",0.14000000000000001,1,"6AG10551CB007BA2"]
["6AG1055-1FB00-7BA2","SIPLUS LOGO! DM8 230 V -40...+70Β°C start up -25Β°C with conformal coating based on 6ED1055-1FB00-0BA2 . Expansion module, PS/I/O: 230V/230V/relay, 2 MW, 4 DI/4 DO for LOGO! 8",185,"ST",1,"LOGO!",0.17499999999999999,1,"6AG10551FB007BA2"]
["6AG1055-1HB00-7BA2","SIPLUS LOGO! DM8 24R -40...+70 Β°C start up -25Β°C with conformal coating based on 6ED1055-1HB00-0BA2 . Expansion module, PS/I/O: 24V/24V/relay, 2 MW 4 DI/4 DO, AC/DC/NPN input for LOGO! 8",185,"ST",1,"LOGO!",0.17499999999999999,1,"6AG10551HB007BA2"]
["6AG1055-1MA00-7BA2","SIPLUS LOGO! AM2 -40...+70Β°C start up -25Β°C with conformal coating based on 6ED1055-1MA00-0BA2 . Expansion module, PS/: 12/24 V DC, 2 AI, 0-10 V or 0/4-20 mA for LOGO! 8",269,"ST",1,"LOGO!",0.14000000000000001,1,"6AG10551MA007BA2"]
["6AG1055-1MB00-7BA2","SIPLUS LOGO! DM8 12/24R -40...+70Β°C start up -25Β°C with conformal coating based on 6ED1055-1MB00-0BA2 . Expansion module, PS/I/O: 12, 24V/12V/24V/relay, 2 MW, 4 DI/4 DO for LOGO! 8",185,"ST",1,"LOGO!",0.17499999999999999,1,"6AG10551MB007BA2"]
["6AG1055-1MD00-7BA2","SIPLUS LOGO! AM2 RTD -40 ... 70Β°C start up -25Β°C with conformal coating based on 6ED1055-1MD00-0BA2 . extens. module, PS: 12/24 V DC, 2AI-50...+200Β°C Pt100/1000 for LOGO! 8",225,"ST",1,"LOGO!",0.13600000000000001,1,"6AG10551MD007BA2"]
["6AG1055-1MM00-7BA2","SIPLUS LOGO! AM2 AQ -40...+70 Β°C start up -25Β°C with conformal coating based on 6ED1055-1MM00-0BA2 . Expansion module, PS: 24 V DC, 2 AO, 0-10 V, 0/4-20 mA for LOGO! 8",326,"ST",1,"LOGO!",0.14000000000000001,1,"6AG10551MM007BA2"]
["6AG1055-1NB10-7BA2","SIPLUS LOGO! DM16 24R -40...+70 Β°C start up -25Β°C with conformal coating based on 6ED1055-1NB10-0BA2 . Expansion module, PS/I/O: 24 V DC/24 V DC/relay, 8 DI/8 DO, 4 MW for LOGO! 8",310,"ST",1,"LOGO!",0.3,1,"6AG10551NB107BA2"]
["6AG1055-4MH08-2BA0","SIPLUS LOGO! TDE -10...+60Β°C start up 0Β°C with conformal coating based on 6ED1055-4MH08-0BA0 . Text Display, 6-line, 3 background colors, 2 Ethernet ports, installation accessories for LOGO! 8",282,"ST",1,"LOGO!",0.32,1,"6AG10554MH082BA0"]
["6AG1057-1AA00-0AA2","Front panel assembly kit 8 MW with keys for LOGO!+SIPLUS extreme",107,"ST",1,"LOGO!",0.17,1,"6AG10571AA000AA2"]
["6AG1057-1AA00-0AA3","Front panel assembly kit 4 MW MT for LOGO!+SIPLUS extreme",62.2,"ST",1,"LOGO!",0.15,1,"6AG10571AA000AA3"]
["6AG1057-1AA02-0AA0","Input simulator for LOGO 12/24 V",219,"ST",1,"SIMATIC",5.7000000000000002E-2,1,"6AG10571AA020AA0"]
["6AG1064-1AA01-0AA0","COMMISSIONING BOX F. SINAMICS S WITH CONNECTING CABLE",765,"ST",1,"SIMATIC",0.79500000000000004,1,"6AG10641AA010AA0"]
["6AG1064-1AA03-0AA0","SINAMICS G110 training case",1862,"ST",1,"SIMATIC",12,1,"6AG10641AA030AA0"]
["6AG1067-0AA10-0AA0","LOGO! KNX display with CMK2000",2841,"ST",1,"SIMATIC",8.1,1,"6AG10670AA100AA0"]
["6AG1067-0AA32-0AA0","Demo setup_S7-1500",712,"ST",1,"SIMATIC",5,1,"6AG10670AA320AA0"]
["6AG1067-0AA33-0AA0","DEMO CASE S7-1200F For Step7 Basic V11",10270,"ST",1,"SIMATIC",24.5,1,"6AG10670AA330AA0"]
["6AG1067-1AA13-0AA0","SINUMERIK 828D simulator PPU281.3 MCP483C PN, I/O module PP 72/48D 2/2A PN SITOP Power Supply 24V 5A, SCALANCE X005",24327,"ST",1,"SIMATIC",30,1,"6AG10671AA130AA0"]
["6AG1067-1AA16-0AA1","SINAMICS S120 power rack",34449,"ST",1,"SIMATIC",120,1,"6AG10671AA160AA1"]
["6AG1067-1AA18-0AA0","SINAMICS S110 demo case SINAMICS S110 servo drive PM240-2 Power Module, 0.37 kW (0.5 hp) CU305 DP Control Unit MULTIMEDIA-CARD 64MB SIMATIC S7-300 controller SIMATIC Touch Panel TP177B,  4.3'β€™ TFT Widescreen Color SIMOTICS S-1FK7 synchronous motor Tanos Systainer case size 4.",12768,"ST",1,"SIMATIC",13.85,1,"6AG10671AA180AA0"]
["6AG1067-1AA23-0AA1","SINUMERIK 840D sl PN Rack",37878,"ST",1,"SIMATIC",56.2,1,"6AG10671AA230AA1"]
["6AG1067-1AA24-0AA1","SINUMERIK 828D Basic with software for Turning and milling",27266,"ST",1,"SIMATIC",30,1,"6AG10671AA240AA1"]
["6AG1067-1AA25-0AA0","SINAMICS G120C training case PROFIBUS in compact design. Components: SINAMICS G120C, 0.55 kW, IOP-2 and BOP-2 and one SIMOTICS induction motor Supply voltage: 230 V 1 AC WxHxD (mm): 315x400x300 Weight: approx. 9 kg Training case G120C is supplied in a stackable case Tanos Systainer Sz. 4 supplied",2596,"ST",1,"SIMATIC",10,1,"6AG10671AA250AA0"]
["6AG1067-1AA32-0AA0","SINAMICS V90 PN Democase 2-axis preparation for S7-1500(T) S7-1500 not included",8033,"ST",1,"SIMATIC",19.2,1,"6AG10671AA320AA0"]
["6AG1067-1AA33-0AA0","Demo case SINAMICS S210 PN 2-axis 100 W Safety Prepared for S7-1500(T) S7-1500 not in scope of delivery .",9813,"ST",1,"SIMATIC",21,1,"6AG10671AA330AA0"]
["6AG1067-2AA00-0AC1","SINAMICS_Democase G120X 1AC 230V GP induction motor 1LE1002 IOP-2 Smart Access Module (SAM) ready for use with Extention module Transportation case with wheels",4556,"ST",1,"SIMATIC",14,1,"6AG10672AA000AC1"]
["6AG1067-2AA00-0AC2","SINAMICS_Democase_G120XA 230V GP induction motor 1LE1002 IOP-2, BOP-2, Smart Access Module (SAM) and transportation case with wheels",4262,"ST",1,"SIMATIC",1E-3,1,"6AG10672AA000AC2"]
["6AG1101-1BB00-4AA3","SIPLUS NET SCALANCE X101-1 for medial exposure based on 6GK5101-1BB00-2AA3",670,"ST",1,"SIMATIC",0.55000000000000004,1,"6AG11011BB004AA3"]
["6AG1106-2BB00-7AC2","SIPLUS NET SCALANCE XC106-2 -40 ... +70Β°C with conformal coating based on 6GK5106-2BB00-2AC2 . SCALANCE XC106-2, unmanaged IE switch, 6x 10/100 Mbit/s RJ45 ports, 2x 100 Mbit/s Multimode BFOC, LED diagnostics, error-signaling contact with set button, redundant Power supply Manual available as a download",1481,"ST",1,"SIMATIC",0.63500000000000001,1,"6AG11062BB007AC2"]
["6AG1107-1BQ40-7AA3","SIPLUS AS-Interface 2AO IP67 -25...+70Β°C with conformal coating based on 3RK1107-1BQ40-0AA3 . AS-Interface compact module, IP67 analog, 2 AO, Number format S7, 2x 1 output (M12), 4...20mA for 2-wire actuators active channels 1 and 2 Mounting plate 3RK1901-0CA00 must be ordered separately",416,"ST",1,"SIMATIC",0.2,1,"6AG11071BQ407AA3"]
["6AG1123-2DB03-2AX0","SIPLUS HMI KTP400 Basic Color PN -20...+60Β°C with conformal coating based on 6AV2123-2DB03-0AX0 . 4\" TFT display, 65536 colors PROFINET\" interface",785,"ST",1,"SIMATIC",0.45900000000000002,1,"6AG11232DB032AX0"]
["6AG1123-2GA03-2AX0","SIPLUS HMI KTP700 Basic DP -20...+50Β°C with conformal coating based on 6AV2123-2GA03-0AX0 . Key/touch \"operation, \"\"7\"\"\"\" TFT display,\" 65536 colors, PROFIBUS interface, configurable as of WinCC Basic V13/ STEP 7 Basic V13, contains open source software, which is provided free of charge See enclosed CD-ROM",1344,"ST",1,"SIMATIC",0.8,1,"6AG11232GA032AX0"]
["6AG1123-2GB03-2AX0","SIPLUS HMI KTP700 Basic Color PN -20...+50Β°C with conformal coating based on \"6AV2123-2GB03-0AX0 . \"\"7\"\"\"\" TFT\" \"display, 65536 colors\"\" PROFINET\" interface",1302,"ST",1,"SIMATIC",0.97699999999999998,1,"6AG11232GB032AX0"]
["6AG1123-2JB03-2AX0","SIPLUS HMI KTP900 Basic Color PN -20...+50Β°C with conformal coating based on \"6AV2123-2JB03-0AX0 . \"\"9\"\"\"\" TFT\" \"display, 65536 colors\"\" PROFINET\" interface",2058,"ST",1,"SIMATIC",1.1299999999999999,1,"6AG11232JB032AX0"]
["6AG1123-2MA03-2AX0","SIPLUS HMI KTP1200 Basic DP -10...+50Β°C with conformal coating based on 6AV2123-2MA03-0AX0 . Key/touch \"operation, \"\"12\"\"\"\" TFT display,\" 65536 colors PROFIBUS interface, configurable as of WinCC Basic V13/ STEP 7 Basic V13, contains open source software, which is provided free of charge See enclosed CD-ROM",2793,"ST",1,"SIMATIC",2.17,1,"6AG11232MA032AX0"]
["6AG1123-2MB03-2AX0","SIPLUS HMI KTP1200 Basic -10...+50Β°C with conformal coating based on 6AV2123-2MB03-0AX0 . Key/touch \"operation, \"\"12\"\"\"\" TFT display,\" 65536 colors PROFINET interface, configurable from WinCC Basic V13/ STEP 7 Basic V13, contains open source software, which is provided free of charge See enclosed CD-ROM",2793,"ST",1,"SIMATIC",2.1619999999999999,1,"6AG11232MB032AX0"]
["6AG1124-0GC01-4AX0","SIPLUS HMI TP700 COMFORT FOR medial stress with conformal coating based on 6AV2124-0GC01-0AX0",1806,"ST",1,"SIMATIC",1.56,1,"6AG11240GC014AX0"]
["6AG1124-0GC13-2AX0","SIPLUS HMI TP700 Comfort Outdoor conformal coating -30 ... +60Β°C based on 6AV2124-0GC13-0AX0 . Comfort \"Panel, Touch operation, 7\"\"\" widescreen TFT display, 16 million colors, PROFINET interfaces, MPI/PROFIBUS DP interface, 12 MB configuration memory, Windows CE 6.0, configurable as of WINCC Comfort V13 SP1, HSP",2720,"ST",1,"SIMATIC",1.5609999999999999,1,"6AG11240GC132AX0"]
["6AG1124-0JC01-4AX0","SIPLUS HMI TP900 Comfort for medial exposure with conformal coating based on 6AV2124-0JC01-0AX0",2972,"ST",1,"SIMATIC",3.3,1,"6AG11240JC014AX0"]
["6AG1124-0MC01-4AX0","SIPLUS HMI TP1200 Comfort for medial exposure with conformal coating based on 6AV2124-0MC01-0AX0",3833,"ST",1,"SIMATIC",3.56,1,"6AG11240MC014AX0"]
["6AG1124-0QC02-4AX1","SIPLUS HMI TP1500 COMFORT FOR medial stress with conformal coating based on 6AV2124-0QC02-0AX1 . Comfort \"Panel, Touch operation, 15\"\"\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",4704,"ST",1,"SIMATIC",7.2,1,"6AG11240QC024AX1"]
["6AG1124-0QC13-2AX0","SIPLUS HMI TP1500 Comfort OD -30 ... +60Β°C with conformal coating based on 6AV2124-0QC13-0AX0 . TP1500 Comfort Outdoor, Comfort Panel, \"Touch, 15\"\"\" Widescreen-TFT-Display, 16 MIO colours, PROFINET interface, MPI/PROFIBUS-DP interface, 12MByte Projektierungsspeicher, Windows CE 6.0, projektierbar ab WinCC Comfort V13 SP1, HSP",7770,"ST",1,"SIMATIC",6.2,1,"6AG11240QC132AX0"]
["6AG1124-0UC02-4AX1","SIPLUS HMI TP1900 Comfort for medial exposure with conformal coating based on 6AV2124-0UC02-0AX1 . Comfort \"Panel, Touch operation, 19\"\"\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",5691,"ST",1,"SIMATIC",8.66,1,"6AG11240UC024AX1"]
["6AG1124-0XC02-4AX1","SIPLUS HMI TP2200 Comfort for medial exposure with conformal coating based on 6AV2124-0XC02-0AX1 . Comfort \"Panel, key operation, 22\"\"\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",6689,"ST",1,"SIMATIC",9.2799999999999994,1,"6AG11240XC024AX1"]
["6AG1124-1DC01-4AX0","SIPLUS HMI KP400 Comfort for medial exposure with conformal coating based on 6AV2124-1DC01-0AX0",1197,"ST",1,"SIMATIC",0.8,1,"6AG11241DC014AX0"]
["6AG1124-1GC01-4AX0","SIPLUS HMI KP700 Comfort for medial exposure with conformal coating based on 6AV2124-1GC01-0AX0",1964,"ST",1,"SIMATIC",5,1,"6AG11241GC014AX0"]
["6AG1124-1JC01-4AX0","SIPLUS HMI KP900 Comfort for medial exposure with conformal coating based on 6AV2124-1JC01-0AX0",3140,"ST",1,"SIMATIC",5,1,"6AG11241JC014AX0"]
["6AG1124-1MC01-4AX0","SIPLUS HMI KP1200 Comfort for medial exposure with conformal coating based on 6AV2124-1MC01-0AX0",3980,"ST",1,"SIMATIC",5,1,"6AG11241MC014AX0"]
["6AG1124-1QC02-4AX1","SIPLUS HMI KP1500 Comfort for medial exposure with conformal coating based on 6AV2124-1QC02-0AX1 . Comfort \"Panel, key operation, 15\"\"\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",5240,"ST",1,"SIMATIC",7.32,1,"6AG11241QC024AX1"]
["6AG1124-2DC01-4AX0","SIPLUS HMI KTP400 Comfort for medial exposure with conformal coating based on 6AV2124-2DC01-0AX0",1197,"ST",1,"SIMATIC",0.79,1,"6AG11242DC014AX0"]
["6AG1131-4BD01-2AA0","SIPLUS ET 200S 4DI (1 PU=5 units) -25...+60Β°C with conformal coating based on 6ES7131-4BD01-0AA0 . Electronic module 24 V DC 15 mm width, 5 units per packing unit",319,"PAK",1,"SIMATIC",0.18,1,"6AG11314BD012AA0"]
["6AG1131-4BD01-7AB0","SIPLUS ET 200S EM 4DI HF -25...+70Β°C based on 6ES7131-4BD01-0AB0 5 units per packing unit",388,"PAK",1,"SIMATIC",0.18,1,"6AG11314BD017AB0"]
["6AG1131-4BF00-7AA0","SIPLUS ET 200S EM 8 DI -25...+70Β°C based on 6ES7131-4BF00-0AA0",92.899999999999991,"ST",1,"SIMATIC",4.2000000000000003E-2,1,"6AG11314BF007AA0"]
["6AG1131-4BF50-7AA0","SIPLUS ET 200S EM 8 DI 24 V DC -40...+70Β°C based on 6ES7131-4BF50-0AA0",92.899999999999991,"ST",1,"SIMATIC",4.2999999999999997E-2,1,"6AG11314BF507AA0"]
["6AG1131-6BF00-7CA0","SIPLUS ET 200SP DI 8x24VDC HF -40...+70Β°C with conformal coating based on 6ES7131-6BF00-0CA0 . digital input module, DI 8x 24 V DC High Feature, suitable for BU type A0, Color code CC01, channel diagnostics",129,"ST",1,"SIMATIC",3.6999999999999998E-2,1,"6AG11316BF007CA0"]
["6AG1131-6BF01-7BA0","SIPLUS ET 200SP, digital input module, DI 8x DC 24V standard, -40...+70Β°C with conformal coating based on 6ES7131-6BF01-0BA0 . type 3 (IEC 61131), sink input, (PNP, P-reading), Packing unit: 1 piece, fits to BU-type A0, Colour Code CC01, input delay time 0,05..20ms, module diagnostics for: short-circuit of sensor supply, wire break, supply voltage",118,"ST",1,"SIMATIC",3.5999999999999997E-2,1,"6AG11316BF017BA0"]
["6AG1131-6BF61-7AA0","SIPLUS ET 200SP, digital input modul, DI 8x DC 24V SRC BA, -40...+70Β°C with conformal coating based on 6ES7131-6BF61-0AA0 . type 1 (IEC 61131), source Input (NPN, M-reading) Packing unit: 1 piece, fits to BU-type A0, Colour Code CC02, input delay time 0,05..20ms, module diagnostics for: supply voltage",93.5,"ST",1,"SIMATIC",3.5000000000000003E-2,1,"6AG11316BF617AA0"]
["6AG1131-6BH01-7BA0","SIPLUS ET 200SP, digital input module, DI 16X DC 24V standard, -40...+70Β°C with conformal coating based on 6ES7131-6BH01-0BA0 . type 3 (IEC 61131), sink input, (PNP, P-reading), Packing unit: 1 Piece, passend fΓΌr BU-Typ A0, Farbcode CC00, Modul-Diagnose input delay time 0,05..20ms, diagnostics wire break, diagnostics supply voltage",153,"ST",1,"SIMATIC",3.6999999999999998E-2,1,"6AG11316BH017BA0"]
["6AG1131-6CF00-7AU0","SIPLUS ET 200SP DI 8x48VUC BA -40...+70Β°C with Conformal Coating based on 6ES7131-6CF00-0AU0 . digital input module, DI 8x 24 V AC..48 V UC Basic, packing quantity: 1 unit, suitable for BU type U0, color code CC20, module diagnostics",158,"ST",1,"SIMATIC",5.8999999999999997E-2,1,"6AG11316CF007AU0"]
["6AG1131-6FD01-7BB1","SIPLUS ET 200SP, Digital input module, DI 4x 120..230V AC ST, type 3 (IEC 61131) -40...+70Β°C with conformal coating based on 6ES7131-6FD01-0BB1 . Packing unit: 1 piece, fits to BU-type B1, Colour Code CC41, module diagnostics",119,"ST",1,"SIMATIC",4.5999999999999999E-2,1,"6AG11316FD017BB1"]
["6AG1131-6TF00-7CA0","SIPLUS ET 200SP -40...+70Β°C start up temperature: -25Β°C with conformal coating based on 6ES7131-6TF00-0CA0 . digital input module, DI 8x NAMUR High Feature, suitable for BU type A0, Color code CC01, channel diagnostics",422,"ST",1,"SIMATIC",0.04,1,"6AG11316TF007CA0"]
["6AG1132-4BB01-2AB0","SIPLUS ET 200S 2DO HF (1 PU=5 units) -25...+60Β°C based on 6ES7132-4BB01-0AB0",263,"PAK",1,"SIMATIC",0.187,1,"6AG11324BB012AB0"]
["6AG1132-4BB31-7AB0","SIPLUS ET 200S 2DO HF -25...+70 Β°C based on 6ES7132-4BB31-0AB0 5 units per packing unit",425,"PAK",1,"SIMATIC",0.19800000000000001,1,"6AG11324BB317AB0"]
["6AG1132-4BD02-7AA0","SIPLUS ET 200S EM 4DO Standard -25...+70Β°C with conformal coating based on 6ES7132-4BD02-0AA0 . Electronic module 24 V DC/0.5A 15 mm width, 5 units per packing unit",364,"PAK",1,"SIMATIC",0.184,1,"6AG11324BD027AA0"]
["6AG1132-4BD32-2AA0","SIPLUS ET 200S EM 4DO 24 V DC/2A -25...+60Β°C with conformal coating based on 6ES7132-4BD32-0AA0 5 units per packing unit",570,"PAK",1,"SIMATIC",0.189,1,"6AG11324BD322AA0"]
["6AG1132-4BF00-7AA0","SIPLUS ET 200S EM 8 DO -25...+70Β°C with conformal coating based on 6ES7132-4BF00-0AA0 . Electronics module for ET 200S, 8 DO 24 V DC/0.5A 15 mm width, 1 unit per packing unit",105,"ST",1,"SIMATIC",4.3999999999999997E-2,1,"6AG11324BF007AA0"]
["6AG1132-4BF50-7AA0","SIPLUS ET 200S EM 8 DO 24 V DC/ 0.5 -25...+70Β°C based on 6ES7132-4BF50-0AA0",104,"ST",1,"SIMATIC",4.4999999999999998E-2,1,"6AG11324BF507AA0"]
["6AG1132-4HB01-2AB0","SIPLUS ET 200S EM 2RO 24 V DC-230 V AC/5 A -25...+70Β°C based on 6ES7132-4HB01-0AB0 5 units per packing unit . 5 electronic modules for ET 200S, 2 DO relay 24 V DC-230 V AC/5 A, 15 mm width, Substitute value output with LED SF (group fault)",396,"PAK",1,"SIMATIC",0.218,1,"6AG11324HB012AB0"]
["6AG1132-4HB12-2AB0","SIPLUS ET 200S EM 2DO RLY 24-48V DC 230V AC/5A -25...+60 Β°C based on 6ES7132-4HB12-0AB0 5 units per packing unit . 24 V-48 V DC/5 A, 24 V-230 V AC/5 A, 15 mm width, Substitute value output",462,"PAK",1,"SIMATIC",0.23,1,"6AG11324HB122AB0"]
["6AG1132-6BD20-7BA0","SIPLUS ET 200SP, digital output module, DQ 4x 24VDC/2A Standard, -40...+70Β°C start up -25Β°C with conformal coating based on 6ES7132-6BD20-0BA0. suitable for BU type A0, Color code CC02, Module diagnostics",123,"ST",1,"SIMATIC",3.6999999999999998E-2,1,"6AG11326BD207BA0"]
["6AG1132-6BD20-7CA0","SIPLUS ET 200SP DQ 4X24VDC/2A -40 ... +70Β°C with conformal coating based on 6ES7132-6BD20-0CA0. DIGITAL OUTPUT MODULE, FITS TO BU-TYPE A0, COLOR CODE CC02, CHANNEL DIAGNOSIS",156,"ST",1,"SIMATIC",3.6999999999999998E-2,1,"6AG11326BD207CA0"]
["6AG1132-6BF00-7CA0","SIPLUS ET 200SP -40...+70Β°C start up temperature: -25Β°C with conformal coating based on 6ES7132-6BF00-0CA0 . digital output module, DQ 8x 24VDC/0.5A High Feature suitable for BU type A0, Color code CC02, channel diagnostics",139,"ST",1,"SIMATIC",3.5999999999999997E-2,1,"6AG11326BF007CA0"]
["6AG1132-6BF01-7BA0","SIPLUS ET 200SP, digital output module, DQ 8x 24VDC/0.5A ST, -40...+70Β°C with conformal coating based on 6ES7132-6BF01-0BA0 . suitable for BU type A0, Color code CC02, Module diagnostics",118,"ST",1,"SIMATIC",3.5999999999999997E-2,1,"6AG11326BF017BA0"]
["6AG1132-6BF61-7AA0","SIPLUS ET 200SP, Digital output module, DQ 8x 24V DC/0,5A Sink Basic -40...+70Β°C with conformal coating based on 6ES7132-6BF60-0AA0 . suitable for BU type A0, Color code CC01",129,"ST",1,"SIMATIC",3.6999999999999998E-2,1,"6AG11326BF617AA0"]
["6AG1132-6BH01-7BA0","SIPLUS ET 200SP, digital output module, DQ 16x 24VDC/0.5A ST -40...+70Β°C with conformal coating based on 6ES7132-6BH01-0BA0 . suitable for BU type A0, Color code CC00, Module diagnostics",176,"ST",1,"SIMATIC",3.6999999999999998E-2,1,"6AG11326BH017BA0"]
["6AG1132-6FD00-7CU0","SIPLUS ET 200SP DQ 4x24..230VAC/2A HF -40...+70 Β°C With conformal coating based on 6ES7132-6FD00-0CU0 . Packing unit: 1 unit Two alternative operating modes: DQ and power control, suitable for BU type U0, color code CC20, channel diagnostics",410,"ST",1,"SIMATIC",5.8999999999999997E-2,1,"6AG11326FD007CU0"]
["6AG1132-6GD51-7BA0","SIPLUS ET 200SP RQ 4x24VDC/2A CO ST -40...+70Β°C with conformal coating based on 6ES7132-6GD51-0BA0 . Signal relay module changeover contact, RQ 4x 24VDC/2A CO ST, suitable for BU type A0, color code CC00, module diagnostics",126,"ST",1,"SIMATIC",3.6999999999999998E-2,1,"6AG11326GD517BA0"]
["6AG1132-6HD01-7BB1","SIPLUS ET 200SP, Relay module, RQ NO 4x 120V DC..230VAC/5A ST -40...70Β°C with conformal coating based on 6ES7132-6HD00-0BB1. suitable for BU type B0 or B1, Module diagnostics",146,"ST",1,"SIMATIC",4.4999999999999998E-2,1,"6AG11326HD017BB1"]
["6AG1134-0GB00-4AY0","SIPLUS PS UPS1100 BATT MOD -15 ... +50Β°C with conformal coating based on 6EP4134-0GB00-0AY0 . SITOP UPS1100 BATTERY MODULE WITH SERVICE- FREE SEALED LEAD BATTERIES FOR SITOP DC-UPS-MODULES 24 V / 7 W",437,"ST",1,"SIMATIC",6.1,1,"6AG11340GB004AY0"]
["6AG1134-3AB00-7AY0","SIPLUS PS UPS1600 10A -25 ... +70Β°C with conformal coating based on 6EP4134-3AB00-0AY0. Uninterruptible power supply input: 24 V DC Output: DC 24 V/10 A",614,"ST",1,"SIMATIC",0.41199999999999998,1,"6AG11343AB007AY0"]
["6AG1134-3AB00-7AY2","SIPLUS PS UPS1600 10A PN -25 ... +70Β°C with conformal coating based on 6EP4134-3AB00-2AY0. uninterruptible power supply with Ethernet/ POFINET interface Input: 24 V DC Output: 24 V DC/10 A",992,"ST",1,"SIMATIC",0.45,1,"6AG11343AB007AY2"]
["6AG1134-4FB01-2AB0","SIPLUS ET 200S EM 2AI Standard U -25...+60Β°C based on 6ES7134-4FB01-0AB0",254,"ST",1,"SIMATIC",4.4999999999999998E-2,1,"6AG11344FB012AB0"]
["6AG1134-4GB01-2AB0","SIPLUS ET 200S EM 2AI STANDARD I -25...+60Β°C based on 6ES7134-4GB01-0AB0",244,"ST",1,"SIMATIC",4.4999999999999998E-2,1,"6AG11344GB012AB0"]
["6AG1134-4GB11-2AB0","SIPLUS ET 200S EM 2AI I-4DMU -25...+60Β°C based on 6ES7134-4GB11-0AB0",244,"ST",1,"SIMATIC",4.4999999999999998E-2,1,"6AG11344GB112AB0"]
["6AG1134-4GB52-2AB0","SIPLUS ET 200S EM 2AI high speed -25...+60Β°C based on 6ES7134-4GB52-0AB0",498,"ST",1,"SIMATIC",0.06,1,"6AG11344GB522AB0"]
["6AG1134-4GD00-2AB0","SIPLUS ET 200S EM 4 AI I 2-wire -25...+70Β°C with conformal coating based on 6ES7134-4GD00-0AB0 . \"Electronic module 4-20 mA; 13\" bit 15 mm width, for 2-wire transducer Cycle time 40 ms/module with SF LED (group fault)",281,"ST",1,"SIMATIC",4.4999999999999998E-2,1,"6AG11344GD002AB0"]
["6AG1134-4JB51-7AB0","SIPLUS ET 200S EM 2AI RTD -25...+70Β°C with conformal coating based on 6ES7134-4JB51-0AB0",432,"ST",1,"SIMATIC",4.3999999999999997E-2,1,"6AG11344JB517AB0"]
["6AG1134-4LB02-2AB0","SIPLUS ET 200S EM 2AI HF -25...+60Β°C with conformal coating based on 6ES7134-4LB02-0AB0 . 2 AI U High Feature for ET 200S, 15 mm width, Cycle time per module: \"0.5 ms, \"\"+/-10 V; 15 bit+sign,\"\"\" \"+/-5 V; 15 bit+sign, 1..5V;\" \"15\"\" bit, Operational limit\" +/-0.1% with SF LED (group fault)",434,"ST",1,"SIMATIC",5.6000000000000001E-2,1,"6AG11344LB022AB0"]
["6AG1134-4MB02-2AB0","SIPLUS ET 200S EM 2 AE I HF -25...+70Β°C with conformal coating based on 6ES7134-4MB02-0AB0 . Electronic module 15 mm Overall width, Cycle time per module: 0.5 ms, \"+/-20 mA; 15 bit+sign, \"\"4..\" \"20mA; 15 bit,\"\" Operational\" limit +/-0.1% with SF LED (group fault)",360,"ST",1,"SIMATIC",4.5999999999999999E-2,1,"6AG11344MB022AB0"]
["6AG1134-4NB01-7AB0","SIPLUS ET 200S EM 2AI TC HF 0...+70Β°C with conformal coating based on 6ES7134-4NB01-0AB0 . 15 mm width, 15 bit+sign with internal temperature Compensation",320,"ST",1,"SIMATIC",4.5999999999999999E-2,1,"6AG11344NB017AB0"]
["6AG1134-4NB51-2AB0","SIPLUS ET 200S EM 2AI RTD HF -25...+60Β°C based on 6ES7134-4NB51-0AB0",353,"ST",1,"SIMATIC",4.5999999999999999E-2,1,"6AG11344NB512AB0"]
["6AG1134-6FF00-2AA1","SIPLUS ET 200SP AI 8xU BASIC -40 ... +60Β°C with conformal coating based on 6ES7134-6FF00-0AA1 . AI 8XU Basic, suitable for BU type A0, A1, Color code CC02, Module diagnostics, 16 bit",384,"ST",1,"SIMATIC",3.9E-2,1,"6AG11346FF002AA1"]
["6AG1134-6GD01-7BA1","SIPLUS ET 200SP analog input module, AI 4XI 2-/4-wire Standard, -40...+70Β°C with conformal coating based on 6ES7134-6GD01-0BA1 . suitable for BU type A0, A1, Color code CC03, Module diagnostics, 16 bit, +/-0.3%",299,"ST",1,"SIMATIC",0.04,1,"6AG11346GD017BA1"]
["6AG1134-6GF00-7AA1","SIPLUS ET 200SP AI 8XI 2-/4-WIRE BA -40...+70Β°C with Conformal Coating based on 6ES7134-6GF00-0AA1 . suitable for BU type A0, A1, Color code CC01, Module diagnostics, 16 bit",426,"ST",1,"SIMATIC",3.6999999999999998E-2,1,"6AG11346GF007AA1"]
["6AG1134-6HB00-2CA1","SIPLUS ET 200SP AI 2XU/I 2/4-W -40...+60Β°C start up temperature:-25Β°C with conformal coating based on 6ES7134-6HB00-0CA1 . Analog input module, AI 2x U/I 2-, 4-wire high Feature, suitable for BU type A0, A1, Color code CC05, channel diagnostics, 16 bit, +/-0.1%",354,"ST",1,"SIMATIC",4.1000000000000002E-2,1,"6AG11346HB002CA1"]
["6AG1134-6HB00-2DA1","SIPLUS ET 200SP, (-40) -25...+60Β°C with conformal coating based on 6ES7134-6HB00-0DA1 . Analog input module, AI 2x U/I 2-, 4-wire high Speed, suitable for BU type A0, A1, Color code CC00, channel diagnostics, 16 bit, +/-0.3%",474,"ST",1,"SIMATIC",0.04,1,"6AG11346HB002DA1"]
["6AG1134-6HD01-7BA1","SIPLUS ET 200SP, Analog input module, AI 4XU/I 2-wire Standard, -40...+70Β°C with conformal coating based on 6ES7134-6HD00-0BA1 . suitable for BU type A0, A1, Color code CC03, Module diagnostics, 16 bit, +/-0.3%",299,"ST",1,"SIMATIC",0.04,1,"6AG11346HD017BA1"]
["6AG1134-6JD00-2CA1","SIPLUS ET 200SP, Analog input module, AI 4xRTD/TC High Feature, -40...+60Β°C start up -25Β°C with conformal coating based on 6ES7134-6JD00-0CA1. suitable for BU type A0, A1, Color code CC00, channel diagnostics, 16 bit, +/-0.1% , 2-/3-/4-wire",385,"ST",1,"SIMATIC",3.9E-2,1,"6AG11346JD002CA1"]
["6AG1134-6JF00-2CA1","SIPLUS ET 200SP AI 8xRTD/TC 2-wire -40...+60Β°C start up 25 Β°C with conformal coating based on 6ES7134-6JF00-0CA1 . Analog input module, AI 8xRTD/TC 2-wire High-Feature Suitable for BU type A0, A1, color code CC00, Channel diagnostics, 16 bit, +/-0.1%",556,"ST",1,"SIMATIC",3.9E-2,1,"6AG11346JF002CA1"]
["6AG1134-6PA20-7BD0","SIPLUS ET 200SP AI EMETER 480VAC ST -40...+70Β°C with conformal coating based on 6ES7134-6PA20-0BD0 . Analog Input MODULE, AI ENERGY METER 480VAC ST, fits to BU-TYPE D0, CHANNEL DIAGNOSIS",371,"ST",1,"SIMATIC",5.3999999999999999E-2,1,"6AG11346PA207BD0"]
["6AG1134-6TD00-2CA1","SIPLUS ET 200SP 4xAI 2-wire 4-20 mA HART -40...+60Β°C start up 25Β°C with conformal coating based on 6ES7134-6TD00-0CA1 . Analog HART input module, AI 4XI 2-wire HART High-Feature suitable for BU type A0, A1, Color code CC03, channel diagnostics, 16 bit, +/-0.3%",852,"ST",1,"SIMATIC",3.6999999999999998E-2,1,"6AG11346TD002CA1"]
["6AG1135-4FB01-2AB0","SIPLUS ET 200S EM 2AO U -25...+60Β°C based on 6ES7135-4fb01-0AB0",254,"ST",1,"SIMATIC",4.4999999999999998E-2,1,"6AG11354FB012AB0"]
["6AG1135-4GB01-2AB0","SIPLUS ET 200S EM 2AO I Standard -25...+70Β°C with conformal coating based on \"6ES7135-4GB01-0AB0 . \"\"+/-20 mA;\" \"13 bit+sign,\"\" \"\"4..20mA; 13 bit\"\"\" Cycle time less than 1 ms with SF LED (group fault)",247,"ST",1,"SIMATIC",4.5999999999999999E-2,1,"6AG11354GB012AB0"]
["6AG1135-4LB02-7AB0","SIPLUS ET 200S 2AO U high feature -25...+60Β°C based on 6ES7135-4LB02-0AB0",300,"ST",1,"SIMATIC",4.5999999999999999E-2,1,"6AG11354LB027AB0"]
["6AG1135-6GB00-7BA1","SIPLUS ET 200SP AQ 2xI Standard -40 ... +70Β°C with conformal coating based on 6ES7135-6GB00-0BA1 . Analog output module, AQ 2xI Standard, Pack quantity: 1 unit, suitable for BU type A0, A1, Color code CC00, Module diagnostics, 16 bit",273,"ST",1,"SIMATIC",3.9E-2,1,"6AG11356GB007BA1"]
["6AG1135-6HB00-2DA1","SIPLUS ET 200SP AQ 2 X U/I HIGH SPEED -40...+60Β°C start up -25Β°C with conformal coating based on 6ES7135-6HB00-0DA1 . Analog output module, AQ 2x U/I High Speed, suitable for BU type A0, A1, Color code CC00, channel diagnostics, 16 bit, +/-0.3%",474,"ST",1,"SIMATIC",3.7999999999999999E-2,1,"6AG11356HB002DA1"]
["6AG1135-6HB00-7CA1","SIPLUS ET 200SP, Analog output -40...+ 70Β°C with conformal coating based on 6ES7135-6HB00-0CA1 . module, AQ 2x U/I High Feature suitable for BU type A0, A1, Color code CC00, channel diagnostics, 16 bit, +/-0.1%",336,"ST",1,"SIMATIC",3.9E-2,1,"6AG11356HB007CA1"]
["6AG1135-6HD00-7BA1","SIPLUS ET 200SP, Analog output module, AQ 4XU/I Standard, -40...+70Β°C start up -25Β°C with conformal coating based on 6ES7135-6HD00-0BA1 . suitable for BU type A0, A1, Color code CC00, Module diagnostics, 16 bit, +/-0.3%",385,"ST",1,"SIMATIC",3.9E-2,1,"6AG11356HD007BA1"]
["6AG1136-6AA00-2CA1","SIPLUS ET 200SP F-AI 4xI 2-/4-wire HF -25...+60Β°C with conformal coating based on 6ES7136-6AA00-0CA1. electronic module ET 200SP, F-AI 4xI(0)4..20mA HF FAILSAFE ANALOG INPUTS up to PL E (ISO 13849) up to SIL 3 (IEC 61508)",1019,"ST",1,"SIMATIC",6.8000000000000005E-2,1,"6AG11366AA002CA1"]
["6AG1136-6BA00-2CA0","SIPLUS ET 200SP F-DI 4/8x24VDC -25...+60Β°C with conformal coating based on 6ES7136-6BA00-0CA0 . Electronic module 8 F-DI HF, PROFIsafe 24 V DC, 15 mm width, up to PL E (ISO 13849-1), SIL3 (IEC 61508)",471,"ST",1,"SIMATIC",0.09,1,"6AG11366BA002CA0"]
["6AG1136-6DB00-2CA0","SIPLUS ET 200SP -25...+60Β°C with conformal coating based on 6ES7136-6DB00-0CA0 . Electronic module, 4 F-DQ PROFIsafe, 24 V DC/2 A, 15 mm width, up to PL E (ISO 13849), up to SIL 3 (IEC 61508)",540,"ST",1,"SIMATIC",9.1999999999999998E-2,1,"6AG11366DB002CA0"]
["6AG1136-6DC00-2CA0","SIPLUS ET 200SP F-DQ 8x24VDC/0.5A PP HF -25...+60Β°C with conformal coating based on 6ES7136-6DC00-0CA0 . 15 MM width, Cat.4, PL e (EN ISO 13849-1) up to SIL 3 (IEC 61508)",573,"ST",1,"SIMATIC",6.8000000000000005E-2,1,"6AG11366DC002CA0"]
["6AG1136-6PA00-2BC0","SIPLUS ET 200SP -25...+60Β°C with conformal coating based on 6ES7136-6PA00-0BC0 . Power Module F-PM-E, PPM PROFIsafe, 24 V DC, safe shutdown of DQ and F-DQ up to PL D, SIL2 or PL E SIL3 2 for safe, dig. inputs, 1 for safe dig. output PPM",615,"ST",1,"SIMATIC",9.9000000000000005E-2,1,"6AG11366PA002BC0"]
["6AG1136-6RA00-2BF0","SIPLUS ET 200SP F-RQ 24 V DC/24-230 V AC/5 A -25...+60Β°C start up -25Β°C with conformal coating based on 6ES7136-6RA00-0BF0 . F-RQ 1x 24 V DC/24..230V AC/5A ST, 20 mm overall width, 1 relay output (2 NO) Summation output current 5 A, load voltage 24 V DC and 24.. 230 V AC, Can be used up to PL E (ISO 13849-1: 2008)/ SIL 3 (IEC 61508: 2010) if control takes place by (e.g. 6AG1136-6DB00-2CA0) F-DQ",204,"ST",1,"SIMATIC",7.1999999999999995E-2,1,"6AG11366RA002BF0"]
["6AG1137-6AA00-2BA0","SIPLUS ET 200SP -40...+60Β°C start up temperature:-25Β°C with conformal coating based on 6ES7137-6AA00-0BA0 . CM PTP communication module for serial connection RS422, RS485 and RS232, Freeport, 3964 (R), USS, MODBUS RTU Master, Slave, 115200 Kbit/s",493,"ST",1,"SIMATIC",0.04,1,"6AG11376AA002BA0"]
["6AG1137-6BD00-2BA0","SIPLUS ET 200SP CM 4XIO-LINK -40...+60Β°C start up temperature: -25Β°C with conformal coating based on 6ES7137-6BD00-0BA0 . CM 4 X IO-LINK ST Communication Module IO-LINK MASTER V1.1",380,"ST",1,"SIMATIC",3.7999999999999999E-2,1,"6AG11376BD002BA0"]
["6AG1138-4CA01-2AA0","SIPLUS ET 200S PM-E 24 V DC with diagnostics -40...+70Β°C with conformal coating based on 6ES7138-4CA01-0AA0",30.700000000000003,"ST",1,"SIMATIC",0.04,1,"6AG11384CA012AA0"]
["6AG1138-4CA50-2AB0","SIPLUS ET 200S PM-E 24V-48V -25...+60Β°C based on 6ES7138-4CA50-0AB0",76,"ST",1,"SIMATIC",4.1000000000000002E-2,1,"6AG11384CA502AB0"]
["6AG1138-4CB11-2AB0","SIPLUS ET 200S PM-E DC/AC -25...+60Β°C with conformal coating based on 6ES7138-4CB11-0AB0 . PM-E power modules 24-48 V DC, 24-230 V AC, with diagnostics and fuse",66.399999999999991,"ST",1,"SIMATIC",4.4999999999999998E-2,1,"6AG11384CB112AB0"]
["6AG1138-4DA04-2AB0","SIPLUS ET 200S EM 1 Count 24 V/ 100 -25...+60Β°C based on 6ES7138-4DA04-0AB0",343,"ST",1,"SIMATIC",5.3999999999999999E-2,1,"6AG11384DA042AB0"]
["6AG1138-4DD01-7AB0","SIPLUS ET 200S EM 2 Pulse -25...+70Β°C with conformal coating based on 6ES7138-4DD01-0AB0 . Electronic module 2-pulse Pulse generator and timer module, 15 mm wide, 2 channels",500,"ST",1,"SIMATIC",0.05,1,"6AG11384DD017AB0"]
["6AG1138-4DF01-7AB0","SIPLUS ET 200S EM 1SI -25...+70 Β°C with conformal coating based on 6ES7138-4DF01-0AB0",514,"ST",1,"SIMATIC",4.5999999999999999E-2,1,"6AG11384DF017AB0"]
["6AG1138-4DF11-7AB0","SIPLUS ET 200S EM 1SI RS232/ 422 -25...+70Β°C with conformal coating based on 6ES7138-4DF11-0AB0 . serial interface 1-channel, 15 mm width, RS232/422, 485 MODBUS/USS",671,"ST",1,"SIMATIC",4.5999999999999999E-2,1,"6AG11384DF117AB0"]
["6AG1138-4FA05-2AB0","SIPLUS ET 200S F-DI 24 V PROFIsafe -25...+60Β°C with conformal coating based on 6ES7138-4FA05-0AB0 . Electronics module for ET 200S, 4/8 F-DI PROFIsafe, 24 V DC, 30 mm overall width, up to Category 4 (EN 954-1)/ SIL3 (IEC 61508)/PLE (ISO 13849), can also be used in PROFINET configuration with IM 151-3 HF",527,"ST",1,"SIMATIC",8.6999999999999994E-2,1,"6AG11384FA052AB0"]
["6AG1138-4FB04-2AB0","SIPLUS ET 200S F-DO 24 V PROFIsafe -25...+60Β°C with conformal coating based on 6ES7138-4FB04-0AB0 . Electronics module for ET 200S, 4 F-DO PROFIsafe, 24 V DC/2 A, 30 mm overall width, up to Category 4 (EN 954-1)/ SIL3 (IEC 61508)/PLE (ISO 13849), can also be used in PROFINET configuration with IM 151-3 HF",607,"ST",1,"SIMATIC",0.1,1,"6AG11384FB042AB0"]
["6AG1138-4HA00-7AB0","SIPLUS ET 200S DP master interface for IM 151-7 CPU -40...+70Β°C with conformal coating based on 6ES7138-4HA00-0AB0",840,"ST",1,"SIMATIC",0.126,1,"6AG11384HA007AB0"]
["6AG1138-6AA00-2BA0","SIPLUS ET 200SP -40...+60Β°C with conformal coating based on 6ES7138-6AA00-0BA0 . TM count 1x 24 V Counter module, 1 channel for 24 V incremental encoder or pulse encoder, 3 DI, 2 DQ",317,"ST",1,"SIMATIC",5.2999999999999999E-2,1,"6AG11386AA002BA0"]
["6AG1138-6AA00-2BA8","SIPLUS WP321 -40 ... +60Β°C with conformal coating based on 7MH4138-6AA00-0BA0. WEIGHING ELECTRONIC (1 CHANNEL) for STRAIN GAUGE LOAD CELLS FULL BRIDGES (1-4 mV/V) for SIMATIC ET200SP, fits to BU-TYPE A0, RS485- INTERFACE for connection of SIWATOOL or a remote DISPLAY",956,"ST",1,"SIMATIC",1E-3,1,"6AG11386AA002BA8"]
["6AG1138-6BA00-2BA0","SIPLUS ET 200SP TM POSINPUT 1 -40 ... +60Β°C with conformal coating based on 6ES7138-6BA00-0BA0. Counter and positioning module for RS422 incremental encoder or SSI absolute value encoder, 2 DI, 2DQ",350,"ST",1,"SIMATIC",5.3999999999999999E-2,1,"6AG11386BA002BA0"]
["6AG1138-6CG00-2BA0","SIPLUS ET 200SP TM TIMER DIDQ 10x24V -40 ... +60Β°C with conformal coating based on 6ES7138-6CG00-0BA0 . time-controlled digital inputs and outputs 4 DI, 6DQ with time stamp Count, PWM, oversampling",429,"ST",1,"SIMATIC",5.1999999999999998E-2,1,"6AG11386CG002BA0"]
["6AG1138-6DB00-2BB1","SIPLUS ET 200SP -40...+60Β°C start up temperature:-25Β°C with conformal coating based on 6ES7138-6DB00-0BB1 . TM Pulse 2x24V PWM and pulse output 2 channels 2 A for proportional valves and DC motors",533,"ST",1,"SIMATIC",5.2999999999999999E-2,1,"6AG11386DB002BB1"]
["6AG1140-4DK04-4AB3","SIPLUS IPC 427D with conformal coating based on 6AG4140-4DK04-3AB0 . SIMATIC IPC427D (Microbox PC), HD graphic onboard, 24 V DC power \"supply; Core I3-3217UE; 2x Gbit\" \"Ethernet (IE/PN); PROFIBUS DP\" \"12; 2 GB with NVRAM; WIN\" \"Embedded Standard 7, 32 bit;\" CFAST 8 GB, without internal \"mass storage; WinAC RTX 2010\" SP2",3759,"ST",1,"SIMATIC",3,1,"6AG11404DK044AB3"]
["6AG1140-4DL04-2AB3","SIPLUS IPC427D -20Β…+55 Β°C With conformal coating based on 6AG4140-4DL04-3AB0 . Microbox PC HD graphic onboard, Core I3-3217UE; 2x Gbit Ethernet (IE/PN); PROFIBUS DP 12; 4 GB with NVRAM; 1x RS 232; without PCIe; Windows Embedded Standard 7, 32-bit CFast 8 GB, without internal mass storage; WinAC RTX 2010 SP2",3570,"ST",1,"SIMATIC",3,1,"6AG11404DL042AB3"]
["6AG1140-4DL04-4AB3","SIPLUS IPC427D 0...+55Β°C with Conformal Coating based on 6AG4140-4DL04-3AB0 . Microbox PC HD Grafik onboard, Core I3-3217UE; 2x Gbit Ethernet (IE/PN); PROFIBUS-DP 12; Wandmontage; 4 GB mit NVRAM; 1x RS-232; ohne PCIE; WIN Embedded Standard 7, 32 Bit CFAST 8 GB, WinAC RTX 2010 SP2",4284,"ST",1,"SIMATIC",3,1,"6AG11404DL044AB3"]
["6AG1141-5BG37-4FA0","SIPLUS IPC427E 0β€¦+55Β°C with Conformal Coating based on 6AG4141-5BG37-0FA0 . HD graphic onboard, 4x USB V3.0 (high current), PCIe (optional), 24 V DC power supply Core i5-6442EQ; 3x Gbit Ethernet (IE/PN); Mounting onto standard rail; 8 GB and NVRAM; 2x RS232/485; without PCIe; Windows 10 IoT Enterprise 2016; Without replaceable mass storage; 240 GB solid-state drive SATA Without SIMATIC software",4725,"ST",1,"SIMATIC",3,1,"6AG11415BG374FA0"]
["6AG1141-5BG44-4CB1","SIPLUS IPC 427E Bundle1 with conformal coating customized only for Continental. SIPLUS IPC427E Bundle for Conti Consisting of: SIPLUS IPC427E and SIPLUS CP 5622PCI Express X1 card",7214,"ST",1,"SIMATIC",3.2650000000000001,1,"6AG11415BG444CB1"]
["6AG1151-1AA06-7AB0","SIPLUS ET 200S IM 151-1 standard -25...+70Β°C with conformal coating based on 6ES7151-1AA06-0AB0 . Interface module incl. termination module Data volume of 244 bytes each \"for inputs and outputs; max. 63\" I/O modules PROFIBUS DP V0 and V1 up to 2 m width can be \"connected; Bus connection via\" 9-pin D-sub",671,"ST",1,"SIMATIC",0.17299999999999999,1,"6AG11511AA067AB0"]
["6AG1151-1BA02-2AB0","SIPLUS ET 200S IM 151 HF -25...+60Β°C based on 6ES7151-1BA02-0AB0",810,"ST",1,"SIMATIC",0.18,1,"6AG11511BA022AB0"]
["6AG1151-3AA23-2AB0","SIPLUS ET 200S IM 151-3 St -25...+60Β°C based on 6ES7151-3AA23-0AB0",630,"ST",1,"SIMATIC",0.20200000000000001,1,"6AG11513AA232AB0"]
["6AG1151-3BA23-7AB0","SIPLUS ET 200S IM 151-3 PN HF -25...+70Β°C with conformal coating based on 6ES7151-3BA23-0AB0 . Interface module Transmission rate 100 \"Mbit/s max. 63 I/O modules \"\"up\" \"to 2 m width connectable;\"\" 2x\" bus connections via RJ45 incl. termination module",728,"ST",1,"SIMATIC",0.2,1,"6AG11513BA237AB0"]
["6AG1151-7AA21-2AB0","SIPLUS ET 200S IM 151-7 CPU -25...+60Β°C with conformal coating based on 6ES7151-7AA21-0AB0 . ET 200S 128 KB work memory with integrated PROFIBUS DP interface (9-pole D-sub socket) as DP slave, without battery SIMATIC MMC required",1176,"ST",1,"SIMATIC",0.25,1,"6AG11517AA212AB0"]
["6AG1151-7FA21-2AB0","SIPLUS ET 200S IM 151-7 F-CPU -25...+60Β°C with conformal coating based on 6ES7151-7FA21-0AB0 . ET 200S 192 KB work memory with integrated PROFIBUS DP Interface (9-pin D-sub, female) AS DP slave, w/o battery SIMATIC MMC required",1701,"ST",1,"SIMATIC",0.25,1,"6AG11517FA212AB0"]
["6AG1151-8AB01-7AB0","SIPLUS ET 200S IM 151-8 PN/DP CPU -40...+70Β°C start up at -25Β°C with conformal coating based on 6ES7151-8AB01-0AB0. 192 KB work memory, int. PROFINET interface (with three RJ45 ports) as IO controller, without Battery MMC required",1470,"ST",1,"SIMATIC",0.379,1,"6AG11518AB017AB0"]
["6AG1151-8FB01-2AB0","SIPLUS ET 200S IM 151-8F PN/DP -25...+60Β°C with conformal coating based on 6ES7151-8FB01-0AB0 . CPU for ET 200S, 256 KB work memory, int. PROFINET interface (with three RJ45 ports) as IO controller/I-device without battery, MMC required",1901,"ST",1,"SIMATIC",0.38,1,"6AG11518FB012AB0"]
["6AG1153-1AA03-2XB0","SIPLUS DP ET200M IM153-1 -40...+70Β°C start up Temp -25Β°C with conformal coating based on 6ES7153-1AA03-0XB0 . INTERFACE FOR ET 200M, FOR MAX. 8 S7-300 MODULES",494,"ST",1,"SIMATIC",0.28199999999999997,1,"6AG11531AA032XB0"]
["6AG1153-2BA10-7XB0","SIPLUS ET 200M IM 153-2 (*BA02) -40...+70Β°C start up temperature:-25Β°C with conformal coating based on 6ES7153-2BA10-0XB0 . Connection ET 200M IM 153-2 High Feature for max. 12 S7-300 modules with redundancy capability, Time stamp. suitable for isochronous mode New features: up to 12 modules can be used Slave Initiative for Drive ES and Switch ES Expanded quantity structure for HART auxiliary variables Operation of the 64-channel modules 32 signals/slot",749,"ST",1,"SIMATIC",0.28399999999999997,1,"6AG11532BA107XB0"]
["6AG1153-4AA01-7XB0","SIPLUS ET 200M IM 153-4 PN IO -25...+70Β°C with conformal coating based on 6ES7153-4AA01-0XB0 . for max. 12 S7-300 modules, extended functions: Isochronous real-time Communication Class 1 and 2, module replacement without PG operation without MMC, maintenance Support of new IO modules",572,"ST",1,"SIMATIC",0.25,1,"6AG11534AA017XB0"]
["6AG1153-4BA00-7XB0","SIPLUS ET 200M IM 153-4 PN IO HF -40...+70Β°C start up temperature:-25Β°C with conformal coating based on 6ES7153-4BA00-0XB0 . DP, Connection ET 200M for max. 12 S7-300 modules, supports fail-safe module, HART modules, shared device, Medium Redundancy Protocol",871,"ST",1,"SIMATIC",0.26,1,"6AG11534BA007XB0"]
["6AG1155-5AA00-2AC0","SIPLUS ET 200MP IM 155-5 PN HF -40...+60 Β°C With conformal coating based on 6ES7155-5AA00-0AC0 . PROFINET IO device interface module IM 155-5 PN HF, for ET 200MP electronic modules; Up to 12 IO modules without PS; Up to 30 IO modules with additional PS; Integrated 2-port switch; RJ45 shared device; MRP; IRT >=0.25 ms; Isochronous mode FW update; IM0...3; Prioritized run-up S2 redundancy; Shared device with 4 controllers",1002,"ST",1,"SIMATIC",0.35599999999999998,1,"6AG11555AA002AC0"]
["6AG1155-5AA01-7AB0","SIPLUS ET 200MP IM 155-5 PN ST -40Β°C to +70Β°C with conformal coating based on 6ES7155-5AA01-0AB0 . PROFINET IO device Interface module IM 155-5 PN ST for ET 200MP \"electronic modules; up to 12 IO\" modules without PS up to 30 IO modules with additional PS \"Integrated 2-port switch; RJ45\" \"shared device; MRP IRT >=0.25\" \"ms; Isochronous mode FW update;\" \"I&M0...3; FSU with 500 ms\"",762,"ST",1,"SIMATIC",0.35899999999999999,1,"6AG11555AA017AB0"]
["6AG1155-5BA00-2AB0","SIPLUS ET 200MP -40...+60Β°C with conformal coating based on 6ES7155-5BA00-0AB0 . PROFIBUS connection IM 155-5 DP ST for max. 12 S7-1500 modules",663,"ST",1,"SIMATIC",0.36,1,"6AG11555BA002AB0"]
["6AG1155-6AA01-7BN0","SIPLUS ET 200SP IM155-6PN ST -40 ... +70Β°C with conformal coating based on 6ES7155-6AA01-0BN0 . Bundle PROFINET IM, IM 155-6PN ST, max. 32 Peripheriemodules and 16 ET 200AL Modules, Single Hot SWAP, Bundle contains: Interface-Module (6AG1155-6AU01-7BN0), Server-Module (6AG1193-6PA00-7AA0), Busadapter BA 2xRJ45 (6AG1193-6AR00-7AA0)",642,"ST",1,"SIMATIC",0.247,1,"6AG11556AA017BN0"]
["6AG1155-6AU01-2CN0","SIPLUS ET 200SP IM155-6PN HF -40...+60Β°C with Conformal Coating based on 6ES7155-6AU01-0CN0 . 2-port interface modul IM155-6PN/2 High Feature, 1 slot for SIMATIC BusAdapter, max. 64 Periphery modules and 16 ET 200AL modules, S2 redundancy, Multi Hot swapping, 0,25ms isochronous mode, server module included",515,"ST",1,"SIMATIC",0.2,1,"6AG11556AU012CN0"]
["6AG1155-6AU01-7BN0","SIPLUS ET 200SP IM155-6PN ST -40 ... +70Β°C with conformal coating based on 6ES7155-6AU01-0BN0 . PROFINET interface module IM 155-6PN standard, max. 32 I/O modules, and 16 ET 200AL modules, single hot swap, incl. server module",456,"ST",1,"SIMATIC",0.20100000000000001,1,"6AG11556AU017BN0"]
["6AG1155-6BA00-7CN0","SIPLUS ET 200SP IM155-6DP HF -40...+70Β°C start up -25Β°C with conformal coating based on 6ES7155-6BA00-0CN0 . bundle PROFIBUS IM, IM 155-6DP HF, max. 32 I/O modules and 16 ET 200AL modules, Multi Hot SWAP, Bundle contains: Interface-Module (6AG1193-6PA00-7AA0), incl. PROFIBUS connector (6AG1155-6BU00-7CN0), Server-Module",563,"ST",1,"SIMATIC",0.23899999999999999,1,"6AG11556BA007CN0"]
["6AG1193-4CA30-2AA0","SIPLUS ET 200S TM-E15C24-A1 -40...+70Β°C with conformal coating based on 6ES7193-4CA30-0AA0 5 units per packing unit . for electronic modules 15 mm width, spring-type terminals 2x4 terminal connections with terminal access to AUX1, AUX1 continuous",78.599999999999994,"PAK",1,"SIMATIC",0.06,1,"6AG11934CA302AA0"]
["6AG1193-4CA40-2AA0","SIPLUS ET 200S TM-E15S26-A1 -40...+70Β°C with conformal coating based on 6ES7193-4CA40-0AA0 5 units per packing unit . for electronic modules 15 mm width, Screw terminals, 2x6 terminal connections with terminal access to AUX1, AUX1 continuous",126,"PAK",1,"SIMATIC",0.48,1,"6AG11934CA402AA0"]
["6AG1193-4CA50-2AA0","SIPLUS ET 200S TM-E15C26-A1 -40...+70Β°C with conformal coating based on 6ES7193-4CA50-0AA0 5 units per packing unit . for electronic modules 15 mm width, Spring-type terminals, 2x6 terminal connections with terminal access to AUX1, AUX1 continuous",126,"PAK",1,"SIMATIC",0.44,1,"6AG11934CA502AA0"]
["6AG1193-4CB10-7AA0","SIPLUS ET 200S TM-E15C23-0 0...+70Β°C with conformal coating based on 6ES7193-4CB10-0AA0 5 units per packing unit . for electronic modules 15 mm width, spring-type terminals 2x3 terminal connections without terminal access to AUX1, AUX1 continuous",87.3,"PAK",1,"SIMATIC",0.29199999999999998,1,"6AG11934CB107AA0"]
["6AG1193-4CB30-2AA0","SIPLUS ET 200S TM-E15C24-01 -40...+70Β°C with conformal coating based on 6ES7193-4CB30-0AA0 5 units per packing unit . for electronic modules 15 mm width, spring-type terminals 2x4 terminal connections without terminal access to AUX1, AUX1 continuous",78.599999999999994,"PAK",1,"SIMATIC",0.3,1,"6AG11934CB302AA0"]
["6AG1193-4CB70-7AA0","SIPLUS ET 200S TM-E15N24-0 -40...+70Β°C with conformal coating based on 6ES7193-4CB70-0AA0 5 units per packing unit . for electronic modules, 15 mm width, FastConnect terminal, 2x4 terminal connections without terminal access to AUX1, AUX1 continuous",96.899999999999991,"PAK",1,"SIMATIC",0.443,1,"6AG11934CB707AA0"]
["6AG1193-4CD20-2AA0","SIPLUS ET 200S TM-P15S23-A0 -40...+70Β°C with conformal coating based on 6ES7193-4CD20-0AA0 . for power modules, 15 mm width, Screw terminals 2x3 terminal connections with terminal access to AUX1, AUX1 interrupted",17.100000000000001,"ST",1,"SIMATIC",7.6999999999999999E-2,1,"6AG11934CD202AA0"]
["6AG1193-4CD30-2AA0","SIPLUS ET 200S TM-P15C23-A0 -40...+70Β°C with conformal coating based on 6ES7193-4CD30-0AA0 . for power modules, 15 mm width, spring-type terminals (Cage Clamp) 2x3 terminal connections with terminal access to AUX1, AUX1 interrupted",17.100000000000001,"ST",1,"SIMATIC",7.0000000000000007E-2,1,"6AG11934CD302AA0"]
["6AG1193-4CE10-2AA0","SIPLUS ET 200S TM-P15C22-01 -40...+70Β°C with conformal coating based on 6ES7193-4CE10-0AA0 . for power modules, 15 mm width, spring-type terminals (Cage Clamp) 2x2 terminal connections without terminal access to AUX1, AUX1 continuous",17.100000000000001,"ST",1,"SIMATIC",6.0999999999999999E-2,1,"6AG11934CE102AA0"]
["6AG1193-4CF50-7AA0","SIPLUS ET 200S TM-E30C46-A1 -40...+70Β°C with conformal coating based on 6ES7193-4CF50-0AA0 . for electronic modules 30 mm overall width, spring-type terminals 4x 6 terminal connections with terminal access to AUX1, AUX1 continuous",50.2,"ST",1,"SIMATIC",0.16,1,"6AG11934CF507AA0"]
["6AG1193-4CG30-2AA0","SIPLUS ET 200S TM-E30C44-01 -40...+70Β°C with conformal coating based on 6ES7193-4CG30-0AA0 . for electronic modules 30 mm overall width, spring-type terminals 4x 4 terminal connections without terminal access to AUX1, AUX1 continuous",59.800000000000004,"ST",1,"SIMATIC",0.12,1,"6AG11934CG302AA0"]
["6AG1193-4CL30-7AA0","SIPLUS ET 200S TM-E15C24-AT 0...+70Β°C with conformal coating based on 6ES7193-4CL30-0AA0 . for electronic module 2 AI TC High Feature, 15 mm width, spring-type terminals with terminal access to AUX1, AUX1 continuous",45.4,"ST",1,"SIMATIC",7.0000000000000007E-2,1,"6AG11934CL307AA0"]
["6AG1193-4JA00-2AA0","SIPLUS ET 200S termination module -25...+60Β°C based on 6ES7193-4JA00-0AA0",42.7,"ST",1,"SIMATIC",2.7E-2,1,"6AG11934JA002AA0"]
["6AG1193-6AA00-0AA0","SIPLUS Mounting Kit ET 200SP",410,"ST",1,"SIMATIC",1E-3,1,"6AG11936AA000AA0"]
["6AG1193-6AF00-7AA0","SIPLUS ET 200SP -40...+70Β°C start up -25Β°C with conformal coating based on 6ES7193-6AF00-0AA0 . Bus Adapter BA 2xFC, 2x FastConnect connections for PROFINET",171,"ST",1,"SIMATIC",6.3E-2,1,"6AG11936AF007AA0"]
["6AG1193-6AG00-2AA0","SIPLUS ET 200SP BA 2XLC -40...+60Β°C with conformal coating based on 6ES7193-6AG00-0AA0 . 2 X LC GLASS-FO-CONNECTORS, for PROFINET",504,"ST",1,"SIMATIC",6.3E-2,1,"6AG11936AG002AA0"]
["6AG1193-6AP00-2AA0","SIPLUS ET 200SP -40...+60Β°C start up -25Β°C with conformal coating based on 6ES7193-6AP00-0AA0 . Bus Adapter BA 2xSCRJ, 2 SCRJ FO connections, for PROFINET",504,"ST",1,"SIMATIC",7.8E-2,1,"6AG11936AP002AA0"]
["6AG1193-6AR00-7AA0","SIPLUS ET 200SP Bus Adapter BA 2xRJ45 -40...+70Β°C with conformal coating based on 6ES7193-6AR00-0AA0 . Bus Adapter BA 2xRJ45 2xRJ45 sockets for PROFINET",215,"ST",1,"SIMATIC",5.5E-2,1,"6AG11936AR007AA0"]
["6AG1193-6BP00-7BA0","SIPLUS ET 200SP, BASEUNIT BU15-P16+A0+2B, BU-TYPE A0, -40... +70Β°C with conformal coating based on 6ES7193-6BP00-0BA0 . PUSH-IN TERMINALS, W/O AUX-TERMINALS, BRIDGED TO LEFT BU WXH: 15MMX117MM",32.5,"ST",1,"SIMATIC",4.9000000000000002E-2,1,"6AG11936BP007BA0"]
["6AG1193-6BP00-7BA1","SIPLUS ET 200SP, BaseUnit BU15-P16+A0+2B/T, BU type A1, -40...+70Β°C start up -25Β°C with conformal coating based on 6ES7193-6BP00-0BA1 . Push-in terminals, with without AUX terminals, bridged to the left, WxH: 15x 117 mm, with temperature acquisition",44.9,"ST",1,"SIMATIC",4.9000000000000002E-2,1,"6AG11936BP007BA1"]
["6AG1193-6BP00-7BD0","SIPLUS ET 200SP -40...+70Β°C with conformal coating based on 6ES7193-6BP00-0BD0. BaseUnit BU20-P12+A0+0B, BU type D0, Push-in terminals, without AUX terminals, bridged to the left, WxH: 20 mmx117 mm",44.6,"ST",1,"SIMATIC",4.9000000000000002E-2,1,"6AG11936BP007BD0"]
["6AG1193-6BP00-7BU0","SIPLUS ET 200SP BU20-P16+A0+2B -40...+70 Β°C With conformal coating based on 6ES7193-6BP00-0BU0 . Base unit type U0, packing quantity: 1 unit Push-in terminals, without auxiliary terminals, bridged to the left, WxH: 20 mm x 117 mm",50.4,"ST",1,"SIMATIC",4.8000000000000001E-2,1,"6AG11936BP007BU0"]
["6AG1193-6BP00-7DA0","SIPLUS ET 200SP, BaseUnit BU15-P16+A0+2D, BU type A0, -40...+70Β°C with conformal coating based on 6ES7193-6BP00-0DA0 . Push-in terminals, without AUX terminals, New load group, WxH: 15x 117 mm",57.4,"ST",1,"SIMATIC",4.9000000000000002E-2,1,"6AG11936BP007DA0"]
["6AG1193-6BP00-7DA1","SIPLUS ET 200SP, based on Unit BU15-P16+A0+2D/T, BU type A1, -40...+70Β°C start up -25Β°C with conformal coating based on 6ES7193-6BP00-0DA1 . Push-in terminals, with without AUX terminals, New load group, WxH: 15x 117 mm, with temperature acquisition",69.899999999999991,"ST",1,"SIMATIC",4.8000000000000001E-2,1,"6AG11936BP007DA1"]
["6AG1193-6BP00-7DU0","SIPLUS ET 200SP BU20-P16+A0+2D -40...+70 Β°C With conformal coating based on 6ES7193-6BP00-0DU0 . BU type U0, packing quantity: 1 unit Push-in terminals, without auxiliary terminals, new potential group, WxH: 20 mm x 117 mm",76.699999999999989,"ST",1,"SIMATIC",4.8000000000000001E-2,1,"6AG11936BP007DU0"]
["6AG1193-6BP20-2BF0","SIPLUS ET 200SP BU20-P8+A4+0B -25...+60Β°C with conformal coating based on 6ES7193-6BP20-0BF0. BaseUnit BU20-P8+A4+0B, BU type F0, Push-in terminals, with 4 AUX terminals, bridged to the left, WxH: 20 mmx117 mm",43.7,"ST",1,"SIMATIC",5.7000000000000002E-2,1,"6AG11936BP202BF0"]
["6AG1193-6BP20-7BA0","SIPLUS ET 200SP, BASEUNIT BU15-P16+A10+2B, BU-TYPE A0, -40 ... +70Β°C with conformal coating based on 6ES7193-6BP20-0BA0 . PUSH-IN TERMINALS, WITH 10 AUX-TERMINALS, BRIDGED TO LEFT BU WXH: 15MMX141MM",43.800000000000004,"ST",1,"SIMATIC",0.06,1,"6AG11936BP207BA0"]
["6AG1193-6BP20-7BB0","SIPLUS ET 200SP -40...+70Β°C with conformal coating based on 6ES7193-6BP20-0BB0. BaseUnit BU20-P12+A4+0B, BU type B0, Push-in terminals, with 4 AUX terminals, bridged to the left, WxH: 20 mmx117 mm",44.6,"ST",1,"SIMATIC",5.7000000000000002E-2,1,"6AG11936BP207BB0"]
["6AG1193-6BP20-7BB1","SIPLUS ET 200SP -40...+70Β°C start up temperature: -25Β°C with conformal coating based on 6ES7193-6BP20-0BB1. BaseUnit BU20-P12+A0+4B, BU type B1, Push-in terminals, without AUX terminals, bridged to the left, WxH: 20 mmx117 mm",45.300000000000004,"ST",1,"SIMATIC",5.7000000000000002E-2,1,"6AG11936BP207BB1"]
["6AG1193-6BP20-7DA0","SIPLUS ET 200SP, BASEUNIT BU15-P16+A10+2D, BU-TYPE A0, -40 ... +70Β°C with conformal coating based on 6ES7193-6BP20-0DA0 . PUSH-IN TERMINALS, WITH 10 AUX-TERMINALS, NEW LOADGROUP, WXH: 15MMX141MM",68.199999999999989,"ST",1,"SIMATIC",5.8999999999999997E-2,1,"6AG11936BP207DA0"]
["6AG1193-6BP20-7DC0","SIPLUS ET 200SP -25...+60Β°C with conformal coating based on 6ES7193-6BP20-0DC0. BaseUnit BU20-P6+A2+4D, BU type C0, Push-in terminals, with 2 AUX terminals, New load group, WxH: 20 mmx117 mm",68.699999999999989,"ST",1,"SIMATIC",4.9000000000000002E-2,1,"6AG11936BP207DC0"]
["6AG1193-6BP40-7BA1","SIPLUS ET 200SP, BaseUnit BU15-P16+A0+12B/T, BU type A1, -40...+70Β°C with conformal coating based on 6ES7193-6BP40-0BA1 . Push-in terminals, with 2x5 add-on terminals, bridged to the left, WxH: 15 mm x 141 mm, with temperature acquisition",55.7,"ST",1,"SIMATIC",0.06,1,"6AG11936BP407BA1"]
["6AG1193-6BP40-7DA1","SIPLUS ET 200SP, based on Unit BU15-P16+A0+12D/T, BU type A1, -40...+70Β°C with conformal coating based on 6ES7193-6BP40-0DA1 . Push-in terminals, with 2x5 add-on terminals, New load group, WxH: 15 mm x 141 mm, with temperature acquisition",80.699999999999989,"ST",1,"SIMATIC",5.8999999999999997E-2,1,"6AG11936BP407DA1"]
["6AG1193-6PA00-7AA0","SIPLUS ET 200SP Server-/ Termination module -40...+70Β°C with conformal coating based on 6ES7193-6PA00-0AA0 . Server module for ET 200SP",90.8,"ST",1,"SIMATIC",2.3E-2,1,"6AG11936PA007AA0"]
["6AG1195-7HA00-2XA0","SIPLUS ET 200M active bus module 1x ps+1x IM 153 -40...+70Β°C based on 6ES7195-7HA00-0XA0",112,"ST",1,"SIMATIC",0.108,1,"6AG11957HA002XA0"]
["6AG1195-7HB00-7XA0","SIPLUS ET 200M active bus module 2x 40 mm modules -40...+70Β°C based on 6ES7195-7HB00-0XA0",242,"ST",1,"SIMATIC",0.13200000000000001,1,"6AG11957HB007XA0"]
["6AG1195-7HC00-2XA0","SIPLUS ET 200M active bus module for holding an 80 mm wide I/O module -40...+70Β°C with conformal coating based on 6ES7195-7HC00-0XA0 . for removal and insertion function",228,"ST",1,"SIMATIC",0.124,1,"6AG11957HC002XA0"]
["6AG1195-7HD10-2XA0","SIPLUS ET 200M active bus module For holding 2 IM 153-2 Red -40...+70Β°C with conformal coating based on 6ES7195-7HD10-0XA0 . for removal and insertion function during RUN operating time",287,"ST",1,"SIMATIC",0.13500000000000001,1,"6AG11957HD102XA0"]
["6AG1195-7HG00-2XA0","SIPLUS ET 200M partition F -25...+60Β°C with conformal coating based on 6ES7195-7HG00-0XA0",202,"ST",1,"SIMATIC",0.115,1,"6AG11957HG002XA0"]
["6AG1195-7KF00-2XA0","SIMATIC S7-300 safety protector -25...+60Β°C with conformal coating based on 6ES7195-7KF00-0XA0 . Safety protector between F and standard modules With redundant ET 200M interface modules, use only with partition",286,"ST",1,"SIMATIC",0.28100000000000003,1,"6AG11957KF002XA0"]
["6AG1197-1LB00-4XA0","SIPLUS S7-400 Y-coupler for medial exposure based on 6ES7197-1lb00-0XA0",617,"ST",1,"SIMATIC",0.25,1,"6AG11971LB004XA0"]
["6AG1202-2BH00-2BA3","SIPLUS NET SCALANCE X202-2PIRT -25...+60Β°C based on 6GK5202-2BH00-2BA3",1680,"ST",1,"SIMATIC",1.05,1,"6AG12022BH002BA3"]
["6AG1204-2BB10-4AA3","SIPLUS NET SCALANCE X204-2 -40...+60Β°C for medial exposure based on 6GK5204-2BB10-2AA3 . Managed IE switch, 4x 10/100 Mbit/s RJ45 ports, 2x 100 Mbit/s multimode BFOC, LED diagnostics, error signaling contact with set button, Redundant power supply, PROFINET IO device, network management, integr. redundancy manager, incl. electron. Manual on CD-ROM, C-plug optional",1523,"ST",1,"SIMATIC",1,1,"6AG12042BB104AA3"]
["6AG1204-2BC10-2AA3","SIPLUS NET SCALANCE X204-2LD -40...+60Β°C with conformal coating based on 6GK5204-2BC10-2AA3",3308,"ST",1,"SIMATIC",1.014,1,"6AG12042BC102AA3"]
["6AG1207-1BQ40-7AA3","SIPLUS AS-Interface 2AI IP67 -25...+70Β°C with conformal coating based on 3RK1207-1BQ40-0AA3 . AS-Interface compact module Number format S7 2x inputs (M12), 4...20 mA for 4-wire sensors active channels 1 and 2 no smoothing filter 50 Hz Mounting plate 3RK1901-0CA00 must be ordered separately, profile 7.3",453,"ST",1,"SIMATIC",0.187,1,"6AG12071BQ407AA3"]
["6AG1207-3BQ40-7AA3","SIPLUS AS-Interface 2AI IP67 -25...+70Β°C with conformal coating based on 3RK1207-3BQ40-0AA3 . AS-Interface compact module, IP67 analog, 2 AI, Number format S7 2x inputs (M12), Pt100 LIN. unit for 4-wire sensors active channels 1 and 2 no smoothing filter 50 Hz Mounting plate 3RK1901-0CA00 must be ordered separately, profile 7.3",407,"ST",1,"SIMATIC",0.183,1,"6AG12073BQ407AA3"]
["6AG1208-0BA10-2AA0","SIPLUS NET SCALANCE X208 -40...+60Β°C with conformal coating based on 6GK5208-0BA10-2AA3 . Managed IE switch, 8x 10/100Mbit/s RJ45 ports, LED diagnostics, error signaling contact with set button, Redundant power supply, PROFINET IO device, network management, integr. redundancy manager, incl. electronic Manual on CD-ROM, C-plug optional",1229,"ST",1,"SIMATIC",1.0429999999999999,1,"6AG12080BA102AA0"]
["6AG1210-1PE14-2UL1","SIPLUS SINAMICS G120 PM 240-2 FSA-1.5kW -20...+50Β°C with conformal coating based on 6SL3210-1PE14-3UL1 . unfiltered with integrated braking chopper 380-480 V 3 AC +10/-10% 47-63 Hz Power high overload: 1.1 kW at 200% 3s, 150% 57s, 100% 240S Power low overload: 1, 5kW 196x 73x 165 (HxWxD), FSA Degree of protection IP20 without Control Unit and operator panel Released as of firmware version V4.6",700,"ST",1,"SIMATIC",1.7,1,"6AG12101PE142UL1"]
["6AG1210-1PE18-2UL1","SIPLUS G120 PM 240-2 FSA-3kW -20...+50Β°C with conformal coating based on 6SL3210-1PE18-0UL1 . unfiltered with integrated braking chopper 380-480 V 3 AC +10/-10% 47-63 Hz Power high overload: 2.2kW at 200% 3s, 150% 57s, 100% 240S Power low overload: 3kW at 150% 3s, 110% 57s, 100% 240S 196x 73x 165 (HxWxD), FSA Degree of protection IP20 without Control Unit and operator panel Released as of firmware version V4.6",840,"ST",1,"SIMATIC",1.7,1,"6AG12101PE182UL1"]
["6AG1210-1PE21-2UL0","SIPLUS G120 PM 240-2 FSB 7.5kW Power Module PM 240-2 unfilt. -20...+50Β°C with conformal coating based on 6SL3210-1PE21-8UL0 . with integrated braking chopper 380-480 V 3 AC +10/-10% 47-63 Hz Power high overload: 5.5kW at 200% 3s,150% 57s,100% 240s Power rating low overload: 7.5 kW at 150% 3s,110% 57s,100% 240s 291x 100x 165 (HxWxD), FSB Degree of protection IP20 without Control Unit and operating unit Released as of firmware version V4.6",1743,"ST",1,"SIMATIC",3,1,"6AG12101PE212UL0"]
["6AG1210-1PE23-2UL0","SIPLUS G120 PM 240-2 FSC 15kW Power Module PM 240-2 unfiltered -20...+50Β°C with conformal coating based on 6SL3210-1PE23-3UL0 . with integrated braking chopper 380-480 V 3 AC +10/-10% 47-63 Hz Power high overload: 11kW at 200% 3s,150% 57s,100% 240s Power low overload: 15kW at 150% 3s,110% 57s,100% 240s 355x 140x 165 (HxWxD), FSC Degree of protection IP20 without Control Unit and operating unit Released as of firmware version V4.6",2793,"ST",1,"SIMATIC",4.8,1,"6AG12101PE232UL0"]
["6AG1210-1PE26-2AL0","SIPLUS PM240-2 -20 to +50Β°C (HO) -20 to +40Β°C (LO) With conformal coating based on 6SL3210-1PE26-0AL0  With integr. class A filter With integr. braking chopper 3AC380-480V+10/-20% 47-63Hz Power high overload: 22 kW at 200% 3s, 150% 57NC, 100% 240s; Power low overload: 30 kW at 150% 3s, 110% 57NC, 100% 240s; 472x 200x 237 (HxWxD), construction type FSD, Degree of protection IP20 Without CU or operating unit released as of CU firmware version V4.7 HF8",5418,"ST",1,"SIMATIC",19,1,"6AG12101PE262AL0"]
["6AG1210-1PE26-2UL0","SIPLUS PM240-2 -20 bis +50Β°C (HO) -20 bis +40Β°C (LO) with conformal coating based on 6SL3210-1PE26-0UL0 . unfilteded with integrated brake-chopper 3AC380-480V+10/-20% 47-63Hz power high overload: 22kW with 200% 3S, 150% 57S, 100% 240S; power low overload: 30kW with 150% 3S, 110% 57S, 100% 240S; 472 X 200 X 237 (HXWXD), FSD protection IP20 without CU and panel approved for CU FW-Version V4.7 HF8",5103,"ST",1,"SIMATIC",18.3,1,"6AG12101PE262UL0"]
["6AG1210-1PE28-2AL0","SIPLUS PM240-2 -20 bis +50Β°C(HO) -20 bis +40Β°C (LO) with conformal coating based on 6SL3210-1PE28-8AL0 . with built in CL. A FILTER with built in braking chopper 3AC380-480V +10/-20% 47-63HZ OUTPUT HIGH OVERLOAD: 37KW FOR 200% 3S, 150% 57S,100% 240S OUTPUT LOW OVERLOAD: 45kW FOR 150% 3S, 110% 57S,100% 240S 551 X 275 X 237 (HXWXD), FSF, PROTECTION IP20 WITHOUT CU AND PANEL APPROVED FOR CU FW-VERSION V4.7 HF8 V4.7 HF8",8043,"ST",1,"SIMATIC",28.38,1,"6AG12101PE282AL0"]
["6AG1210-1PE28-2UL0","SIPLUS PM240-2 -20 bis +50Β°C(HO) -20 bis +40Β°C (LO) with conformal coating based on 6SL3210-1PE28-8UL0 . unfiltered with built in braking chopper 3AC380-480V +10/-20% 47-63HZ OUTPUT HIGH OVERLOAD: 37KW FOR 200% 3S, 150% 57S,100% 240S OUTPUT LOW OVERLOAD: 45kW FOR 150% 3S, 110% 57S,100% 240S 551 X 275 X 237 (HXWXD), FSF, PROTECTION IP20 WITHOUT CU AND PANEL APPROVED FOR CU FW-VERSION V4.7 HF8 V4.7 HF8",7560,"ST",1,"SIMATIC",26.4,1,"6AG12101PE282UL0"]
["6AG1210-1PE31-2AL0","SIPLUS PM240-2 -20 bis +50Β°C (HO) -20 bis +40Β°C (LO) with conformal coating based on 6SL3210-1PE31-5UL0 . with integrated class a filter with integrated brake-chopper 3AC380-480V+10/-20% 47-63Hz power high overload: 55kW with 200% 3S, 150% 57S, 100% 240S; power low overload: 75kW with 150% 3S, 75% 57S, 100% 240S; 708x 305x 357 (HxBxT), FSF protection IP20 without CU and panel approved for CU FW- Version V4.7 HF8",10815,"ST",1,"SIMATIC",64,1,"6AG12101PE312AL0"]
["6AG1210-1PE31-2UL0","SIPLUS PM240-2 -20 to +50 Β°C (HO) -20 to +40 Β°C (LO) With conformal coating based on 6SL3210-1PE31-5UL0 . Unfiltered with integrated braking chopper 380-480 V 3 AC +10/-20% 47-63 Hz Power high overload: 55 kW with 200% 3s, 150% 57s, 100% 240S; Power low overload: 75 kW with 150% 3s, \"110% 57S, 100% 240s;\" 708x 305x 357 (HxWxD), FSF IP20 degree of protection without CU and operating unit released as of CU FW Version V4.7 HF8",10112,"ST",1,"SIMATIC",58,1,"6AG12101PE312UL0"]
["6AG1210-1PE32-2AL0","SIPLUS PM240-2 -20 bis +50Β°C (HO) -20 bis +40Β°C (LO) with conformal coating based on 6SL3210-1PE32-5AL0 . with builtin CL. A FILTER with built in braking chopper 3AC380-480V +10/-20% 47-63HZ OUTPUT HIGH OVERLOAD: 110KW FOR 200% 3S,150% 57S,100% 240S OUTPUT LOW OVERLOAD: 132kW FOR 150% 3S, 110% 57S,100% 240S 708 X 305 X 357 (HXWXD), FSF PROTECTION IP20 WITHOUT CU AND PANEL APPROVED FOR CU FW- VERSION V4.7 HF8 V4.7 HF8",15330,"ST",1,"SIMATIC",66,1,"6AG12101PE322AL0"]
["6AG1210-1PE32-2UL0","SIPLUS PM240-2 -20 bis +50Β°C (HO) -20 bis +40Β°C (LO) with conformal coating based on 6SL3210-1PE32-5UL0 . with builtin CL. A FILTER with built in braking chopper 3AC380-480V +10/-20% 47-63HZ OUTPUT HIGH OVERLOAD: 110KW FOR 200% 3S,150% 57S,100% 240S OUTPUT LOW OVERLOAD: 132kW FOR 150% 3S, 110% 57S,100% 240S 708 X 305 X 357 (HXWXD), FSF PROTECTION IP20 WITHOUT CU AND PANEL APPROVED FOR CU FW- VERSION V4.7 HF8 V4.7 HF8",14385,"ST",1,"SIMATIC",62,1,"6AG12101PE322UL0"]
["6AG1212-1AE40-2XB0","SIPLUS S7-1200 CPU 1212C DC/DC/DC -40...+70Β°C with conformal coating based on 6ES7212-1AE40-0XB0 . compact \"CPU, DC/DC/DC, onboard I/O: \"\"8\" \"DI 24 V DC;\"\" \"\"6 DO 24 V DC;\"\" 2\" AI 0-10 V DC, Power supply: 20.4-28.8V DC, Program/data memory 75 KB",435,"ST",1,"SIMATIC",0.35599999999999998,1,"6AG12121AE402XB0"]
["6AG1212-1AE40-4XB0","SIPLUS S7-1200 CPU 1212C DC/DC/DC for medial exposure with conformal coating based on 6ES7212-1AE40-0XB0 . compact CPU, DC/DC/DC, onboard I/O: 8 DI 24 V DC 6 DO 24 V DC 2 AI 0-10 V DC, Power supply: 20.4-28.8V DC Program/data memory 50 KB",344,"ST",1,"SIMATIC",0.34,1,"6AG12121AE404XB0"]
["6AG1212-1BE40-2XB0","SIPLUS S7-1200 CPU 1212C AC/DC/relay -40...+70Β°C with conformal coating based on 6ES7212-1BE40-0XB0 . compact CPU, AC/DC/relay, onboard I/O: 8 DI 24 V DC 6 DO relay 2 A 2 AI 0-10 V DC, Power supply: 85-264 V AC at 47-63 Hz, Program/data memory 75 KB",435,"ST",1,"SIMATIC",0.41599999999999998,1,"6AG12121BE402XB0"]
["6AG1212-1BE40-4XB0","SIPLUS S7-1200 CPU 1212C AC/DC/relay for medial exposure with conformal coating based on 6ES7212-1BE40-0XB0 . compact CPU, AC/DC/relay, onboard I/O: 8 DI 24 V DC 6 DO relay 2 A 2 AI 0-10 V DC, Power supply: AC 85-264V AC @ 47-63 Hz, Program/data memory 75 KB",344,"ST",1,"SIMATIC",0.38800000000000001,1,"6AG12121BE404XB0"]
["6AG1212-1HE40-2XB0","SIPLUS S7-1200 CPU 1212C DC/DC/relay -40...+70Β°C with conformal coating based on 6ES7212-1HE40-0XB0 . onboard \"I/O: \"\"8 DI 24 V DC; 6 DO relay\" \"2 A;\"\" 2 AI 0-10 V DC, Power\" supply: DC 20.4-28.8V DC, Program/data memory 75 KB",435,"ST",1,"SIMATIC",0.35399999999999998,1,"6AG12121HE402XB0"]
["6AG1212-1HE40-4XB0","SIPLUS S7-1200 CPU 1212C DC/DC/relay for medial exposure with conformal coating based on 6ES7212-1HE40-0XB0 . compact CPU, DC/DC/relay, onboard I/O: 8 DI 24 V DC 6 DO relay 2A 2 AI 0-10 V DC Power supply: 20.4-28.8 V DC Program/data memory 75 KB",344,"ST",1,"SIMATIC",0.35399999999999998,1,"6AG12121HE404XB0"]
["6AG1212-2BB00-4AA3","SIPLUS NET SCALANCE X212-2 for medial exposure with conformal coating based on 6GK5212-2BB00-2AA3 . Managed IE switch, 12x 10/100Mbit/s RJ45 ports, 2x 100 Mbit/s multimode BFOC, LED diagnostics, error signaling contact with set button, Redundant power supply, PROFINET IO device, network management, integr. redundancy manager, incl. electron. Manual on CD-ROM, C-plug optional",2793,"ST",1,"SIMATIC",1.54,1,"6AG12122BB004AA3"]
["6AG1214-1AF40-5XB0","SIPLUS S7-1200 CPU 1214FC DC/DC/DC -25...+55Β°C with conformal coating based on 6ES7214-1AF40-0XB0 . compact \"CPU, DC/DC/DC, \"\"onboard I/O: 14\" \"DI 24 V DC;\"\" \"\"10 DO 24 V DC; 2\" \"AI 0-10 V DC,\"\" Power supply: DC\" 20.4-28.8 V DC Program/data memory 125 KB",821,"ST",1,"SIMATIC",0.433,1,"6AG12141AF405XB0"]
["6AG1214-1AG40-2XB0","SIPLUS S7-1200 CPU 1214C DC/DC/DC -40....+70Β°C with conformal coating based on 6ES7214-1AG40-0XB0 . compact CPU, DC/DC/DC, onboard I/O: 14 DI 24 V DC 10 DO 24 V DC 2 AI 0-10 V DC, Power supply: DC 20.4-28.8V DC, Program/data memory 100 KB",658,"ST",1,"SIMATIC",0.41199999999999998,1,"6AG12141AG402XB0"]
["6AG1214-1AG40-4XB0","SIPLUS S7-1200 CPU 1214C DC/DC/DC for medial exposure with conformal coating based on 6ES7214-1AG40-0XB0 . compact CPU, DC/DC/DC, onboard I/O: 14 DI 24 V DC 10 DO 24 V DC 2 AI 0-10 V DC, Power supply: DC 20.4-28.8V DC, Program/data memory 100 KB",518,"ST",1,"SIMATIC",0.41199999999999998,1,"6AG12141AG404XB0"]
["6AG1214-1AG40-5XB0","SIPLUS S7-1200 CPU 1214C DC/DC/DC -40...+60Β°C with conformal coating based on 6ES7214-1AG40-0XB0 signal board usable. compact CPU, \"DC/DC/DC, onboard I/O: \"\"14 DI\" \"24 V DC; 10 DO 24 V DC;\"\" 2 AI\" 0-10 V DC, Power supply: DC 20.4-28.8V DC, Program/data memory 100 KB",578,"ST",1,"SIMATIC",0.41199999999999998,1,"6AG12141AG405XB0"]
["6AG1214-1BG40-2XB0","SIPLUS S7-1200 CPU 1214C AC/DC/relay -40...+70Β°C with conformal coating based on 6ES7214-1BG40-0XB0 . compact CPU, AC/DC/relay, onboard I/O: 14 DI 24 V DC 10 DO relay 2 A 2 AI 0-10 V DC, Power supply: AC 85-264 V AC @ 47-63 Hz, Program/data memory 100 KB",658,"ST",1,"SIMATIC",0.49099999999999999,1,"6AG12141BG402XB0"]
["6AG1214-1BG40-4XB0","SIPLUS S7-1200 CPU 1214C AC/DC/relay for medial exposure with conformal coating based on 6ES7214-1BG40-0XB0 . compact CPU, AC/DC/relay, onboard I/O: 14 DI 24 V DC 10 DO relay 2 A 2 AI 0-10 V DC, Power supply: AC 85-264 V AC @ 47-63 Hz, Program/data memory 100 KB",518,"ST",1,"SIMATIC",0.49099999999999999,1,"6AG12141BG404XB0"]
["6AG1214-1BG40-5XB0","SIPLUS S7-1200 CPU 1214C AC/DC/relay -40...+60Β°C with conformal coating Signal board usable based on 6ES7214-1BG40-0XB0 . compact CPU, AC/DC/relay, onboard I/O: \"14 DI 24 V DC; 10 DO relay 2 A;\" 2 AI 0-10 V DC, Power supply: AC 85-264 V AC @ 47-63 Hz, Program/data memory 100 KB",578,"ST",1,"SIMATIC",0.49099999999999999,1,"6AG12141BG405XB0"]
["6AG1214-1HF40-5XB0","SIPLUS S7-1200 CPU 1214FC DC/DC/relay -25...+55Β°C with conformal coating based on 6ES7214-1HF40-0XB0 . compact \"CPU, DC/DC/relay, \"\"onboard I/O:\" \"14 DI 24 V DC;\"\" \"\"10 DO relay 2\" \"A;\"\" 2 AI 0-10 V DC, Power\" supply: DC 20.4-28.8 V DC Program/data memory 125 KB",821,"ST",1,"SIMATIC",0.45200000000000001,1,"6AG12141HF405XB0"]
["6AG1214-1HG40-2XB0","SIPLUS S7-1200 CPU 1214C DC/DC/relay -40...+70Β°C with conformal coating based on 6ES7214-1HG40-0XB0 . compact CPU, DC/DC/relay, onboard I/O: 14 DI 24 V DC 10 DO relay 2 A 2 AI 0-10 V DC, Power supply: DC 20.4-28.8V DC, Program/data memory 100 KB",658,"ST",1,"SIMATIC",0.45200000000000001,1,"6AG12141HG402XB0"]
["6AG1214-1HG40-4XB0","SIPLUS S7-1200 CPU 1214C DC/DC/relay for medial exposure with conformal coating based on 6ES7214-1HG40-0XB0 . compact CPU, DC/DC/relay, onboard I/O: 14 DI 24 V DC 10 DO relay 2 A 2 AI 0-10 V DC, Power supply: DC 20.4-28.8V DC, Program/data memory 100 KB",518,"ST",1,"SIMATIC",0.45200000000000001,1,"6AG12141HG404XB0"]
["6AG1214-1HG40-5XB0","SIPLUS S7-1200 CPU 1214C DC/DC/relay -40...+60Β°C with conformal coating Signal board usable based on 6ES7214-1HG40-0XB0 . compact CPU, DC/DC/relay, onboard I/O: \"14 DI 24 V DC; 10 DO relay 2\" \"A; 2 AI 0-10 V DC, Power\" supply: AC 20.4-28.8V DC, Program/data memory 100 KB",578,"ST",1,"SIMATIC",0.45200000000000001,1,"6AG12141HG405XB0"]
["6AG1215-1AF40-5XB0","SIPLUS S7-1200 CPU 1215FC DC/DC/DC -25Β°C...55Β°C with conformal coating based on 6ES7215-1AF40-0XB0 . compact CPU, DC/DC/DC, 2 PROFINET PORT, \"ONBOARD I/O: 14 DI 24VDC; 10 DO\" \"24V DC 0.5A; 2 AI 0-10V DC, 2\" AO 0-20MA DC, POWER SUPPLY: DC 20.4 - 28.8 V DC, PROGRAM/DATA MEMORY 150 KB",1103,"ST",1,"SIMATIC",0.46700000000000003,1,"6AG12151AF405XB0"]
["6AG1215-1AG40-2XB0","SIPLUS S7-1200 CPU 1215C DC/DC/DC -40...+70Β°C with conformal coating based on 6ES7215-1AG40-0XB0 . compact CPU, DC/DC/DC, 2 PROFINET ports, onboard I/O: 14 DI 24 V DC 10 DO 24 V DC 0.5 A 2 AI 0-10 V DC, 2 AO 0-20 mA DC, Power supply: DC 20.4-28.8V DC, Program/data memory 125 KB",986,"ST",1,"SIMATIC",0.44600000000000001,1,"6AG12151AG402XB0"]
["6AG1215-1AG40-4XB0","SIPLUS S7-1200 CPU 1215C DC/DC/DC with conformal coating based on 6ES7215-1AG40-0XB0 . compact CPU, DC/DC/DC, 2 PROFINET ports, onboard I/O: 14 DI 24 V DC 10 DO 24 V DC 0.5 A 2 AI 0-10 V DC, 2 AO 0-20 mA DC, Power supply: DC 20.4-28.8V DC, Program/data memory 125 KB",785,"ST",1,"SIMATIC",0.44600000000000001,1,"6AG12151AG404XB0"]
["6AG1215-1AG40-5XB0","SIPLUS S7-1200 CPU 1215C DC/DC/DC -40...+60Β°C with conformal coating based on 6ES7215-1AG40-0XB0 . compact CPU, DC/DC/DC, 2 PROFINET \"ports, onboard I/O: \"\"14 DI 24 V\" \"DC; 10 DO 24 V DC;\"\" 2 AI 0-10 V\" DC, 2 AO 0-20 mA DC, Power supply: DC 20.4-28.8V DC, Program/data memory 125 KB",879,"ST",1,"SIMATIC",0.46700000000000003,1,"6AG12151AG405XB0"]
["6AG1215-1BG40-2XB0","SIPLUS S7-1200 CPU 1215C AC/DC/relay -40...+70Β°C with conformal coating based on 6ES7215-1BG40-0XB0 . compact CPU, AC/DC/relay, 2 PROFINET Port,onboard I/O: 14 DI 24 VDC 10 DO relay 2 A 2 AI 0-10 VDC 2 AO 0-20 mA DC Power supply: 85-264V AC @ 47-63 Hz, Program/data memory 125 KB",959,"ST",1,"SIMATIC",0.503,1,"6AG12151BG402XB0"]
["6AG1215-1BG40-4XB0","SIPLUS S7-1200 CPU 1215C AC/DC/relay for medial exposure with conformal coating based on 6ES7215-1BG40-0XB0 . compact CPU, AC/DC/relay, onboard I/O: 14 DI 24 V DC 10 DO relay 2 A 2 AI 0-10 V DC 2 AO 0-20 mA DC Power supply: 85-264V AC @ 47-63 Hz, Program/data memory 125 KB",785,"ST",1,"SIMATIC",0.503,1,"6AG12151BG404XB0"]
["6AG1215-1BG40-5XB0","SIPLUS S7-1200 CPU 1215C AC/DC/relay -40...+60Β°C with conformal coating based on 6ES7215-1BG40-0XB0 . compact CPU, AC/DC/relay, 2 PROFINET \"ports onboard I/O: \"\"14 DI 24 V\" \"DC; 10 DO relay 2 A; 2 AI 0-10\" V DC, 2 AO 0-20 mA DC Power supply: AC 85-264 V AC @ 47-63 Hz, Program/data memory 125 KB",851,"ST",1,"SIMATIC",0.52300000000000002,1,"6AG12151BG405XB0"]
["6AG1215-1HG40-2XB0","SIPLUS S7-1200 CPU 1215C DC/DC/relay -40...+70Β°C with conformal coating based on 6ES7215-1HG40-0XB0 . compact CPU, DC/DC/relay, 2 PROFINET ports, onboard I/O: 14 DI 24 V DC 10 DO relay 2 A, 2 AI 0-10 V DC 2 AO 0-20 mA DC, Power supply: DC 20.4-28.8V DC, Program/data memory 125 KB",976,"ST",1,"SIMATIC",0.47299999999999998,1,"6AG12151HG402XB0"]
["6AG1215-1HG40-4XB0","SIPLUS S7-1200 CPU 1215C DC/DC/relay for medial exposure with conformal coating based on 6ES7215-1HG40-0XB0 . compact CPU, DC/DC/relay, 2 PROFINET ports, onboard I/O: 14 DI 24 V DC 10 DO relay 2 A, 2 AI 0-10 V DC 2 AO 0-20 mA DC, Power supply: DC 20.4-28.8V DC, Program/data memory 125 KB",785,"ST",1,"SIMATIC",0.47299999999999998,1,"6AG12151HG404XB0"]
["6AG1215-1HG40-5XB0","SIPLUS S7-1200 CPU 1215C DC/DC/relay -40...+60Β°C with conformal coating Signal board usable based on 6ES7215-1HG40-0XB0 . compact CPU, DC/DC/relay, 2 PROFINET \"ports, onboard I/O: \"\"14 DI 24 V\" \"DC; 10 DO relay 2 A; 2 AI 0-10\" V DC, Power supply: DC 20.4-28.8V DC, Program/data memory 125 KB",871,"ST",1,"SIMATIC",0.47499999999999998,1,"6AG12151HG405XB0"]
["6AG1221-1BF32-2XB0","SIPLUS S7-1200 SM 1221 8DI -25...+70Β°C with conformal coating based on 6ES7221-1BF32-0XB0 . Digital input 8 DI, 24 V DC, Sink/Source",181,"ST",1,"SIMATIC",0.17,1,"6AG12211BF322XB0"]
["6AG1221-1BF32-4XB0","SIPLUS S7-1200 SM 1221 8DI for medial exposure with conformal coating based on 6ES7221-1BF32-0XB0 . Digital input 8 DI, 24 V DC, Sink/Source",147,"ST",1,"SIMATIC",0.17,1,"6AG12211BF324XB0"]
["6AG1221-1BH32-2XB0","SIPLUS S7-1200 SM 1221 16DI -25...+70Β°C with conformal coating based on 6ES7221-1BH32-0XB0 . Digital input 16 DI, 24 V DC, Sink/Source",401,"ST",1,"SIMATIC",0.21,1,"6AG12211BH322XB0"]
["6AG1221-1BH32-4XB0","SIPLUS S7-1200 SM 1221 16DI, with conformal coating based on 6ES7221-1BH32-0XB0 . 16 DI, 24 V DC, Sink/Source",237,"ST",1,"SIMATIC",0.21,1,"6AG12211BH324XB0"]
["6AG1221-3AD30-5XB0","SIPLUS S7-1200 SB1221 4DI -40...+60Β°C start up -25Β°C with conformal coating based on 6ES7221-3AD30-0XB0 . Digital inputs 4 DI 5 V DC 200 kHz",122,"ST",1,"SIMATIC",3.5000000000000003E-2,1,"6AG12213AD305XB0"]
["6AG1221-3BD30-5XB0","SIPLUS S7-1200 SB1221 4DI -40...+60Β°C start up -25Β°C with conformal coating based on 6ES7221-3BD30-0XB0 . Digital inputs 4 DI 24 V DC 200 kHz",134,"ST",1,"SIMATIC",3.2000000000000001E-2,1,"6AG12213BD305XB0"]
["6AG1222-1AD30-5XB0","SIPLUS S7-1200 SB1222 I/O -40...+60Β°C start up -25Β°C with conformal coating based on 6ES7222-1AD30-0XB0 . Digital input/output 2 DI/2DO, 5V DC 200kHz",122,"ST",1,"SIMATIC",3.3000000000000002E-2,1,"6AG12221AD305XB0"]
["6AG1222-1BD30-5XB0","SIPLUS S7-1200 SB1222 4DO -40...+60Β°C start up -25Β°C with conformal coating based on 6ES7222-1BD30-0XB0 . Digital output 4 DO 24 V DC 200 kHz",134,"ST",1,"SIMATIC",3.5000000000000003E-2,1,"6AG12221BD305XB0"]
["6AG1222-1BF32-2XB0","SIPLUS S7-1200 SM 1222 8DQ -25...+70Β°C with conformal coating based on 6ES7222-1BF32-0XB0 . Digital output 8 DQ, 24 V DC, transistor 0.5 A",181,"ST",1,"SIMATIC",0.18,1,"6AG12221BF322XB0"]
["6AG1222-1BF32-4XB0","SIPLUS S7-1200 SM 1222 8DQ for medial exposure with conformal coating based on 6ES7222-1BF32-0XB0 . Digital output 8 DQ, 24 V DC, transistor 0.5 A",147,"ST",1,"SIMATIC",0.18,1,"6AG12221BF324XB0"]
["6AG1222-1BH32-2XB0","SIPLUS S7-1200 SM 1222 16DQ -25...+70Β°C with conformal coating based on 6ES7222-1BH32-0XB0 . Digital output 16 DQ, 24 V DC, transistor 0.5 A",287,"ST",1,"SIMATIC",0.22,1,"6AG12221BH322XB0"]
["6AG1222-1BH32-4XB0","SIPLUS S7-1200 SM 1222 16DQ for medial exposure with conformal coating based on 6ES7222-1BH32-0XB0 . Digital output 16 DQ, 24 V DC, transistor 0.5 A",237,"ST",1,"SIMATIC",0.22,1,"6AG12221BH324XB0"]
["6AG1222-1HF32-2XB0","SIPLUS S7-1200 SM 1222 8DQ RLY -25...+70Β°C with conformal coating based on 6ES7222-1HF32-0XB0 . Digital output 8 DQ, relay 2 A",202,"ST",1,"SIMATIC",0.19,1,"6AG12221HF322XB0"]
["6AG1222-1HF32-4XB0","SIPLUS S7-1200 SM 1222 8DQ RLY for medial exposure with conformal coating based on 6ES7222-1HF32-0XB0 . Digital output 8 DQ, relay 2 A",147,"ST",1,"SIMATIC",0.19,1,"6AG12221HF324XB0"]
["6AG1222-1HH32-2XB0","SIPLUS S7-1200 SM 1222 16DQ RLY -25...+70Β°C with conformal coating based on 6ES7222-1HH32-0XB0 . Digital output 16 DQ, relay 2 A",287,"ST",1,"SIMATIC",0.26,1,"6AG12221HH322XB0"]
["6AG1222-1HH32-4XB0","SIPLUS S7-1200 SM 1222 16DQ RLY for medial exposure with conformal coating based on 6ES7222-1HH32-0XB0 . Digital output 16 DQ, relay 2 A",237,"ST",1,"SIMATIC",0.26,1,"6AG12221HH324XB0"]
["6AG1222-1XF32-2XB0","SIPLUS S7-1200 SM 1232 -40....+70Β°C with conformal coating based on 6ES7222-1XF32-0XB0 . S7-1200, digital output SM 1222, 8 DQ, relay CO contact",272,"ST",1,"SIMATIC",0.372,1,"6AG12221XF322XB0"]
["6AG1222-1XF32-4XB0","SIPLUS S7-1200 SM 1222 8DQ with conformal coating based on 6ES7222-1XF32-0XB0 . Digital output SM 1222, 8DQ, Relay Changeover contact",256,"ST",1,"SIMATIC",0.372,1,"6AG12221XF324XB0"]
["6AG1223-0BD30-4XB0","SIPLUS S7-1200 SB1223 2DI/2DO for medial exposure with conformal coating based on 6ES7223-0BD30-0XB0 . Digital input/output 2 DI 24 V DC/2 DO 24 V DC",86.399999999999991,"ST",1,"SIMATIC",0.1,1,"6AG12230BD304XB0"]
["6AG1223-0BD30-5XB0","SIPLUS S7-1200 SB1223 2DI/2DO -40...+60Β°C start up -25Β°C with conformal coating based on 6ES7223-0BD30-0XB0 . Digital input/output 2 DI 24 V DC/2 DO 24 V DC",107,"ST",1,"SIMATIC",0.1,1,"6AG12230BD305XB0"]
["6AG1223-1BH32-2XB0","SIPLUS S7-1200 SM 1223 8DI/8DQ -25...+70Β°C with conformal coating based on 6ES7223-1BH32-0XB0 . Digital input/output SM 1223, 8 DI/8 DO, 8 DI 24 V DC, Sink/Source, 8 DO, transistor 0.5 A",381,"ST",1,"SIMATIC",0.21,1,"6AG12231BH322XB0"]
["6AG1223-1BH32-4XB0","SIPLUS S7-1200 SM 1223 8DI/8DQ for medial exposure with conformal coating based on 6ES7223-1BH32-0XB0 . Digital input/output 8 DI/8 DQ, 8 DI 24 V DC, Sink/Source, 8 DQ, transistor 0.5 A",237,"ST",1,"SIMATIC",0.21,1,"6AG12231BH324XB0"]
["6AG1223-1BL32-2XB0","SIPLUS S7-1200 SM 1223 16 DI/16 DQ -25...+70Β°C with conformal coating based on 6ES7223-1BL32-0XB0 . Digital input/output 16 DI/16 DQ, 16 DI 24 V DC, Sink/Source, 16 DQ, transistor 0.5 A",536,"ST",1,"SIMATIC",0.31,1,"6AG12231BL322XB0"]
["6AG1223-1BL32-4XB0","SIPLUS S7-1200 SM 1223 16 DI/16 DQ for medial exposure with conformal coating based on 6ES7223-1BL32-0XB0 . Digital input/output 16 DI/16 DQ, 16 DI 24 V DC, Sink/Source, 16 DQ, transistor 0.5 A",374,"ST",1,"SIMATIC",0.31,1,"6AG12231BL324XB0"]
["6AG1223-1PH32-2XB0","SIPLUS S7-1200 SM 1223 8DI/8DQ/relay -25...+70Β°C with conformal coating based on 6ES7223-1PH32-0XB0 . Digital input/output 8 DI/8 DQ, 8 DI 24 V DC, Sink/Source, 8 DQ, relay 2:00 AM",287,"ST",1,"SIMATIC",0.21,1,"6AG12231PH322XB0"]
["6AG1223-1PH32-4XB0","SIPLUS S7-1200 SM 1223 8DI/8DQ RLY for medial exposure with conformal coating based on 6ES7223-1PH32-0XB0 . Digital input/output 8 DI/8 DQ, 8 DI 24 V DC, Sink/Source, 8 DQ, relay 2:00 AM",237,"ST",1,"SIMATIC",0.21,1,"6AG12231PH324XB0"]
["6AG1223-1PL32-2XB0","SIPLUS S7-1200 SM 1223 16 DI/16 DQ RLY -25...+70Β°C with conformal coating based on 6ES7223-1PL32-0XB0 . Digital input/output 16 DI/16 DQ, 16 DI 24 V DC, Sink/Source, 16 DQ, relay 2 A",510,"ST",1,"SIMATIC",0.23,1,"6AG12231PL322XB0"]
["6AG1223-1PL32-4XB0","SIPLUS S7-1200 SM 1223 16 DI/16 DQ RLY for medial exposure with conformal coating based on 6ES7223-1PL32-0XB0 . Digital input/output 16 DI/16 DQ, 16 DI 24 V DC, Sink/Source, 16 DQ, relay 2 A",374,"ST",1,"SIMATIC",0.23,1,"6AG12231PL324XB0"]
["6AG1223-1QH32-2XB0","SIPLUS S7-1200 SM 1223 -40...+70Β°C with conformal coating based on 6ES7223-1QH32-0XB0 . SIMATIC S7-1200, Digital inputs/ output SM 1223, 8 DI AC/8 DO RLY, 8 DI 120/230 V AC, 8 DO relay 2 A",461,"ST",1,"SIMATIC",0.21,1,"6AG12231QH322XB0"]
["6AG1223-1QH32-4XB0","SIPLUS S7-1200 SM 1223 8DI/DQ with conformal coating based on 6ES7223-1QH32-0XB0 . SIMATIC S7-1200, Digital inputs/ output SM 1223, 8 DI AC/8 DO RLY, 8 DI 120/230 V AC, 8 DO relay 2 A",382,"ST",1,"SIMATIC",0.21,1,"6AG12231QH324XB0"]
["6AG1223-3AD30-5XB0","SIPLUS S7-1200 SB1223 I/O -40...+60Β°C start up -25Β°C with conformal coating based on 6ES7223-3AD30-0XB0 . Digital input/output 2 DI/2DO, 5V DC 200kHz",122,"ST",1,"SIMATIC",3.5999999999999997E-2,1,"6AG12233AD305XB0"]
["6AG1223-3BD30-5XB0","SIPLUS S7-1200 SB1223 I/O -40...+60Β°C start up -25Β°C with conformal coating based on 6ES7223-3BD30-0XB0 . Digital input/output 2 DI/2DO, 24 V DC 200 kHz",152,"ST",1,"SIMATIC",3.5000000000000003E-2,1,"6AG12233BD305XB0"]
["6AG1226-6BA32-5XB0","SIPLUS S7-1200 SM 1226 F-DI 16x24 V DC -25...+55Β°C with conformal coating based on 6ES7226-6BA32-0XB0 F-DI 16X 24 V DC, PROFIsafe, 70 mm overall width, up to PL E (ISO 13849-1)/ SIL3 (IEC 61508)",346,"ST",1,"SIMATIC",0.09,1,"6AG12266BA325XB0"]
["6AG1226-6DA32-5XB0","SIPLUS S7-1200 SM 1226 F-DQ 4x24 V DC -25...+55Β°C with conformal coating based on 6ES7226-6DA32-0XB0 . F-DQ 4x 24 V DC 2A, PROFIsafe, 70 mm overall width, up to PL E (ISO 13849-1)/ SIL3 (IEC 61508)",346,"ST",1,"SIMATIC",0.09,1,"6AG12266DA325XB0"]
["6AG1226-6RA32-5XB0","SIPLUS S7-1200 SM 1226 F-DQ 2x relay -25...+55Β°C with conformal coating based on 6ES7226-6RA32-0XB0 . F-DQ 2x RLY 5A, PROFIsafe, 70 mm overall width, up to PL E (ISO 13849-1)/ SIL3 (IEC 61508)",465,"ST",1,"SIMATIC",0.09,1,"6AG12266RA325XB0"]
["6AG1231-4HD32-4XB0","SIPLUS S7-1200 SM 1231 4 AI 13 bits for medial exposure with conformal coating based on 6ES7231-4HD32-0XB0 . Analog input, 4 AI, +/-10 V, +/-5 V, +/-2.5 V, or 0-20 mA 12-bit+ sign bit (13 bit ADC)",304,"ST",1,"SIMATIC",0.17199999999999999,1,"6AG12314HD324XB0"]
["6AG1231-4HF32-4XB0","SIPLUS S7-1200 SM 1231 8AI with conformal coating based on 6ES7231-4HF32-0XB0 . Analog input SM 1231, 8 AI, +/-10 V, +/-5 V, +/-2.5 V, or 0-20 mA/4-20 mA, 12 bit+sign or (13 bit ADC)",490,"ST",1,"SIMATIC",0.21199999999999999,1,"6AG12314HF324XB0"]
["6AG1231-5ND32-4XB0","SIPLUS S7-1200 SM 1231 4AI with conformal coating based on 6ES7231-5ND32-0XB0 Analog input, SM 1231, 4 AI, +/-10 V, +/-5 V, +/-2.5 V, +/-1.25 or 0-20 mA/4-20 mA, 15 bit+sign bit",490,"ST",1,"SIMATIC",0.16500000000000001,1,"6AG12315ND324XB0"]
["6AG1231-5PA30-5XB0","SIPLUS S7-1200 SB 1231 1AI RTD -40 ... +60Β°C, start up -25Β°C, with conformal coating based on 6ES7231-5PA30-0XB0 . SIPLUS S7-1200, analog input, SB 1231RTD, 1 AI RTD, PT 100 and PT1000",150,"ST",1,"SIMATIC",3.5000000000000003E-2,1,"6AG12315PA305XB0"]
["6AG1231-5PD32-2XB0","SIPLUS S7-1200 SM 1231 RTD -40...+70Β°C with conformal coating based on 6ES7231-5PD32-0XB0 . SIMATIC S7-1200, Analog input, SM 1231 RTD, 4xAI RTD module",498,"ST",1,"SIMATIC",0.20699999999999999,1,"6AG12315PD322XB0"]
["6AG1231-5PD32-4XB0","SIPLUS S7-1200 SM 1231 with conformal coating based on 6ES7231-5PD32-0XB0 . Analog input, SM 1231 RTD 4xAI RTD module",461,"ST",1,"SIMATIC",0.20699999999999999,1,"6AG12315PD324XB0"]
["6AG1231-5PF32-2XB0","SIPLUS S7-1200 SM 1231 RTD 8AI -25...+70Β°C with conformal coating based on 6ES7231-5PF32-0XB0 . Analog input, SM 1231 RTD, 8xAI RTD module",734,"ST",1,"SIMATIC",0.29599999999999999,1,"6AG12315PF322XB0"]
["6AG1231-5PF32-4XB0","SIPLUS S7-1200 SM 1231 RTD 8AI with conformal coating based on 6ES7231-5PF32-0XB0 . Analog input, SM 1231 RTD, 8xAI RTD module",718,"ST",1,"SIMATIC",0.29599999999999999,1,"6AG12315PF324XB0"]
["6AG1231-5QD32-4XB0","SIPLUS S7-1200 SM 1231 TC with conformal coating based on 6ES7231-5QD32-0XB0 . Analog input, 4 AI thermocouples",429,"ST",1,"SIMATIC",0.16900000000000001,1,"6AG12315QD324XB0"]
["6AG1231-5QF32-4XB0","SIPLUS S7-1200 SM 1231 TC 8AI with conformal coating based on 6ES7231-5QF32-0XB0 . Analog input, SM 1231 TC 8 AI thermocouples",613,"ST",1,"SIMATIC",0.21099999999999999,1,"6AG12315QF324XB0"]
["6AG1232-4HA30-4XB0","SIPLUS S7-1200 SB1232 1AO for medial exposure with conformal coating based on 6ES7232-4HA30-0XB0 . ANALOG OUTPUT 1 AO, +/-10 V DC (12 bit resol.) or 0-20mA (11 bit resol.)",130,"ST",1,"SIMATIC",0.1,1,"6AG12324HA304XB0"]
["6AG1232-4HA30-5XB0","SIPLUS S7-1200 SB1232 1AO -40...+60Β°C start up -25Β°C with conformal coating based on 6ES7232-4HA30-0XB0 . ANALOG OUTPUT 1 AO, +/-10 V DC (12 bit resol.) or 0-20mA (11 bit resol.)",152,"ST",1,"SIMATIC",0.2,1,"6AG12324HA305XB0"]
["6AG1232-4HB32-4XB0","SIPLUS S7-1200 SM 1232 2AQ for medial exposure with conformal coating based on 6ES7232-4HB32-0XB0 . Analog output +/-10 V: 14-bit resolution or 0-20mA: 13-bit resolution",322,"ST",1,"SIMATIC",0.16900000000000001,1,"6AG12324HB324XB0"]
["6AG1232-4HD32-2XB0","SIPLUS S7-1200 SM 1232 -40...+70Β°C with conformal coating based on 6ES7232-4HD32-0XB0 . S7-1200, Analog output, SM 1232, 4 AO, +/-10 V, 14-bit resolution: or 0-20 mA, 13-bit resolution:",728,"ST",1,"SIMATIC",0.214,1,"6AG12324HD322XB0"]
["6AG1232-4HD32-4XB0","SIPLUS S7-1200 SM 1232 4AQ with conformal coating based on 6ES7232-4HD32-0XB0 . SIMATIC S7-1200, Analog output, SM 1232, 4 AO, +/-10 V, 14-bit resolution, or 0-20 mA, 13-bit resolution",566,"ST",1,"SIMATIC",0.214,1,"6AG12324HD324XB0"]
["6AG1234-4HE32-2XB0","SIPLUS S7-1200 SM 1234 4AI/2AQ -25...+70Β°C with conformal coating based on 6ES7234-4HE32-0XB0 . analog I/O +/-10 V: 14-bit resolution 0-20 mA: 13-bit resolution",543,"ST",1,"SIMATIC",0.218,1,"6AG12344HE322XB0"]
["6AG1234-4HE32-4XB0","SIPLUS S7-1200 SM 1234 4AI/2AQ for medial exposure with conformal coating based on 6ES7234-4HE32-0XB0 . analog I/O +/-10 V: 14-bit resolution or 0-20mA: 13-bit resolution",441,"ST",1,"SIMATIC",0.218,1,"6AG12344HE324XB0"]
["6AG1241-1AH32-2XB0","SIPLUS S7-1200 CM1241 RS232 -25...+70Β°C with conformal coating based on 6ES7241-1AH32-0XB0 . Communication module RS232, 9-pole D-sub (socket), supports Freeport",292,"ST",1,"SIMATIC",0.156,1,"6AG12411AH322XB0"]
["6AG1241-1AH32-4XB0","SIPLUS S7-1200cm 1241, with conformal coating based on 6ES7241-1AH32-0XB0 . Communication module RS232, 9-pole D-sub (pin), supports Freeport",192,"ST",1,"SIMATIC",0.156,1,"6AG12411AH324XB0"]
["6AG1241-1CH30-5XB1","SIPLUS S7-1200 CB 1241, -40...+60Β°C start-up -25Β°C with conformal coating based on 6ES7241-1CH30-1XB0 RS 485",133,"ST",1,"SIMATIC",3.3000000000000002E-2,1,"6AG12411CH305XB1"]
["6AG1241-1CH32-2XB0","SIPLUS S7-1200 CM1241 -40...+70 Β°C with conformal coating based on 6ES7241-1CH32-0XB0. Communication module CM 1241, RS422/485, 9-pole D-sub (pin) supports Freeport",301,"ST",1,"SIMATIC",0.159,1,"6AG12411CH322XB0"]
["6AG1241-1CH32-4XB0","SIPLUS S7-1200 CM1241 with conformal coating based on 6ES7241-1CH32-0XB0 . Communication module CM 1241, RS422/485, 9-pole D-sub (pin) supports Freeport",263,"ST",1,"SIMATIC",0.159,1,"6AG12411CH324XB0"]
["6AG1242-5DX30-2XE0","SIPLUS S7-1200CM 1242-5 -25...+55 Β°C with conformal coating based on 6GK7242-5DX30-0XE0 . Communication module CM 1242-5, for connecting S7-1200 to PROFIBUS as DP Slave module",567,"ST",1,"SIMATIC",0.3,1,"6AG12425DX302XE0"]
["6AG1242-6TM10-2BB1","SIPLUS ET 200SP TM ECC 2xPWM ST; -30...60 Β°C With conformal coating Based on 6FE1242-6TM10-0BB1 . Charging controller for conductive charging of electric vehicles according to IEC 61851 with 2 charge outputs; -30 Β°C...60 Β°C 2x Control Pilot; 2x plug Preset; 2x DQ switching contact For load contactor as open collector; 2x DI for feedback message; Load contactor or connector lock; 2x ACT for connector lock Suitable for BU type BU20-P12+A0+4B and BU20-P12+A4+0B",620,"ST",1,"SIMATIC",0.04,1,"6AG12426TM102BB1"]
["6AG1242-7KX31-7XE0","SIPLUS NET CP 1242-7 V2 -40...+70 Β°C with conformal coating based on 6GK7242-7KX31-0XE0 . Communications processor CP 1242-7 V2 for connection of SIMATIC S7-1200 to GSM/GPRS network; Web server access to CPU, data point configuration Observe national approvals",975,"ST",1,"SIMATIC",0.20100000000000001,1,"6AG12427KX317XE0"]
["6AG1243-1BX30-2AX0","SIPLUS S7-1200 CP 1243-1 -40...+70Β°C with conformal coating based on 6GK7243-1BX30-0XE0 . Communications Processor CP 1243-1 for connecting SIMATIC S7-1200 as additional Ethernet interface and for connection to control center via remote system protocols (DNP3, IEC 60870, TeleControl Basic), Security (Firewall, VPN)",1015,"ST",1,"SIMATIC",0.17899999999999999,1,"6AG12431BX302AX0"]
["6AG1243-2AA30-7XB0","SIPLUS S7-1200 CM 1243-2 -25...+70Β°C with conformal coating based on 3RK7243-2AA30-0XB0. S7-1200, CM 1243-2 Communication module AS-Interface master referred to AS-i Specification V3.0",641,"ST",1,"SIMATIC",0.153,1,"6AG12432AA307XB0"]
["6AG1243-5DX30-2XE0","SIPLUS S7-1200cm 1243-5 -25...+55 Β°C with conformal coating based on 6GK7243-5DX30-0XE0 Communication module CM 1243-5, for connecting S7-1200 to PROFIBUS as DP master module",536,"ST",1,"SIMATIC",0.3,1,"6AG12435DX302XE0"]
["6AG1244-0BB12-2BA1","SIPLUS G120 CU240E-2 USS Control Unit CU240E-2 USS -20...+55Β°C with conformal coating based on 6SL3244-0BB12-1BA1. Control Unit CU240E-2 Type with Safety integrated STO RS485 interface, USS protocol 6DI, 3 DO, 2AI,2AO, max. 1F-DI PTC/KTY interface USB and SD/MMC interface Degree of protection IP20 without Power Module",506,"ST",1,"SIMATIC",0.49,1,"6AG12440BB122BA1"]
["6AG1244-0BB12-2FA0","SIPLUS G120 CU240E-2 PN Control Unit CU240E-2 PN -20...+55Β°C with conformal coating based on 6SL3244-0BB12-1FA0 . E-type with Safety Integrated STO PROFINET 6DI, 3DO, 2 AI, 2 AO, max. 1F-DI PTC/KTY interface USB and SD/MMC interface Degree of protection IP20 without Power Module",633,"ST",1,"SIMATIC",0.49,1,"6AG12440BB122FA0"]
["6AG1244-0BB12-2PA1","SIPLUS G120 CU240E-2 DP Control Unit CU240E-2 DP -20...+55Β°C with conformal coating based on 6SL3244-0BB12-1PA1 . E-type with Safety Integrated STO PROFINET 6DI, 3DO, 2 AI, 2 AO, max. 1F-DI PTC/KTY interface USB and SD/MMC interface Degree of protection IP20 without Power Module",633,"ST",1,"SIMATIC",0.49,1,"6AG12440BB122PA1"]
["6AG1255-0AA00-2JA2","SIPLUS G120 IOP-2 -20... +50Β°C with conformal coating based on 6SL3255-0AA00-4JA2. for SIPLUS SINAMICS G120 Language settings: German, English, French, Italian, Spanish, Portuguese, Dutch, Swedish, Russian, Czech, Polish, Turkish Finnish, Chinese simplified",368,"ST",1,"SIMATIC",0.16,1,"6AG12550AA002JA2"]
["6AG1277-1AA10-4AA0","SIPLUS NET CSM 1277 with conformal coating based on 6GK7277-1AA10-0AA0 . Compact Switch Module CSM 1277 Connection SIMATIC S7-1200 and up to 3 further nodes to Industrial Ethernet with 10/100 Mbit/s",273,"ST",1,"SIMATIC",0.2,1,"6AG12771AA104AA0"]
["6AG1278-4BD32-2XB0","SIPLUS S7-1200 SM 1278 IO-Link -25...+70Β°C with conformal coating based on 6ES7278-4BD32-0XB0 . Signal module SM 1278 4xIO-Link Master IO-Link Master V1.1",435,"ST",1,"SIMATIC",0.19700000000000001,1,"6AG12784BD322XB0"]
["6AG1278-4BD32-4XB0","SIPLUS S7-1200 SM 1278 IO-Link with conformal coating based on 6ES7278-4BD32-0XB0 . Signal module SM 1278 4xIO-Link Master IO-Link Master V1.1",311,"ST",1,"SIMATIC",0.19700000000000001,1,"6AG12784BD324XB0"]
["6AG1305-1BA80-2AA0","SIPLUS S7-300 PS 305 -25...+70 Β°C with conformal coating according to EN 50155 T1 Cat 1 Cl A/B based on 6ES7305-1BA80-0AA0 . Stabilized power supplies Input: 24-110 V DC Output: 24 V DC/2 A",408,"ST",1,"SIMATIC",0.8,1,"6AG13051BA802AA0"]
["6AG1307-1EA01-7AA0","SIPLUS S7-300 PS 307 -25 ... +70Β°C with conformal coating based on 6ES7307-1EA01-0AA0 . STABILIZED POWER SUPPLY INPUT: 120/230 V AC OUTPUT: 24 V DC/5 A.",293,"ST",1,"SIMATIC",0.6,1,"6AG13071EA017AA0"]
["6AG1307-1KA02-7AA0","SIPLUS S7-300 PS 307 10 A -25...+70Β°C with conformal coating based on 6ES7307-1KA02-0AA0 . Stabilized power supply PS 307 Input: 120/230 V AC Output: 24 V DC/10 A",366,"ST",1,"SIMATIC",0.8,1,"6AG13071KA027AA0"]
["6AG1308-2FL10-4AA3","SIPLUS NET SCALANCE X308-2 -10...+60 Β°C with conformal coating based on 6GK5308-2FL10-2AA3",3812,"ST",1,"SIMATIC",0.75,1,"6AG13082FL104AA3"]
["6AG1312-5BF04-7AB0","SIPLUS S7-300 CPU 312C for medial exposure -25...+70Β°C based on 6ES7312-5BF04-0AB0 . Compact CPU with MPI, 10 DI/6 DQ, 2 high-speed counters (10 kHz) Integr. power supply 24 V DC, work memory 64 KB, Front connector (1x 40-pole) and Micro Memory Card required",954,"ST",1,"SIMATIC",0.47,1,"6AG13125BF047AB0"]
["6AG1313-5BG04-7AB0","SIPLUS S7-300 CPU 313C for medial exposure -25...+70Β°C based on 6ES7313-5BG04-0AB0 . Compact CPU with MPI, 24 DI/16 DO, 4 AI, 2 AO, 1 Pt100, 3 high-speed counters (30 kHz), Integr. power supply 24 V DC, work memory 128 KB, Front connector (2x 40-pole) and Micro Memory Card required",1890,"ST",1,"SIMATIC",0.72699999999999998,1,"6AG13135BG047AB0"]
["6AG1313-6CG04-7AB0","SIPLUS S7-300 CPU 313C-2DP for medial exposure -25...+70Β°C based on 6ES7313-6CG04-0AB0 . Compact CPU with MPI, 16 DI/16 DO, 3 high-speed counters (30 kHz), integrated DP interface, Integr. power supply 24 V DC, work memory 128 KB, Front connector (1x 40-pole) and Micro Memory Card required",2604,"ST",1,"SIMATIC",0.629,1,"6AG13136CG047AB0"]
["6AG1314-1AG14-2AY0","SIPLUS S7-300 CPU 314 -25...+60 Β°C with conformal coating according to EN 50155 based on 6ES7314-1AG14-0AB0 . Central processing unit with MPI, Integr. power supply 24 V DC, work memory 128 KB, Micro Memory Card required",1218,"ST",1,"SIMATIC",0.28000000000000003,1,"6AG13141AG142AY0"]
["6AG1314-1AG14-7AB0","SIPLUS S7-300 CPU 314 -25...+70 Β°C with conformal coating based on 6ES7314-1AG14-0AB0 . Central processing unit with MPI, Integr. power supply 24 V DC, work memory 128 KB, Micro Memory Card required",1061,"ST",1,"SIMATIC",0.28000000000000003,1,"6AG13141AG147AB0"]
["6AG1314-6BH04-7AB0","SIPLUS S7-300 CPU 314C for medial exposure -25...+70Β°C based on 6ES7314-6BH04-0AB0. Compact CPU with MPI, 24 DI/16 DO, 4 AI, 2 AO, 1 Pt100, 4 high-speed counters (60 kHz), integrated interface RS485, Integr. power supply 24 V DC, work memory 192 KB, Front connector (2x 40-pole) and Micro Memory Card required",2667,"ST",1,"SIMATIC",0.74399999999999999,1,"6AG13146BH047AB0"]
["6AG1314-6CH04-7AB0","SIPLUS S7-300 CPU 314C-2DP for medial exposure -25...+70Β°C based on 6ES7314-6CH04-0AB0 . Compact CPU with MPI, 24 DI/16 DO, 4 AI, 2 AO, 1 Pt100, 4 high-speed counters (60 kHz), integrated DP interface, Integr. power supply 24 V DC, work memory 192 KB, Front connector (2x 40-pole) and Micro Memory Card required",3591,"ST",1,"SIMATIC",0.73799999999999999,1,"6AG13146CH047AB0"]
["6AG1314-6EH04-7AB0","SIPLUS S7-300 CPU 314C-2PN/DP with conformal coating -25...+70Β°C based on 6ES7314-6EH04-0AB0 . Compact CPU with 192 KB work memory, 24 DI/16 DO, 4 AI, 2 AO, 1 Pt100, 4 high-speed counters (60 kHz), 1st interface MPI/DP 12Mbit/ s, 2nd interface Ethernet PROFINET, with 2-port switch, Integr. power supply 24 V DC, Front connector (2x 40-pole) and Micro Memory Card required",3150,"ST",1,"SIMATIC",0.81299999999999994,1,"6AG13146EH047AB0"]
["6AG1315-2AH14-7AB0","SIPLUS S7-300 CPU 315-2DP -25...+70Β°C with conformal coating based on 6ES7315-2AH14-0AB0 . Central processing unit with MPI Integr. power supply 24 V DC Work memory 256 KB 2nd interface DP master/ slave Micro Memory Card required",2573,"ST",1,"SIMATIC",0.34399999999999997,1,"6AG13152AH147AB0"]
["6AG1315-2EH14-7AB0","SIPLUS S7-300 CPU315-2PN/DP -25 ... +70Β°C with conformal coating based on 6ES7315-2EH14-0AB0 . CENTRAL PROCESSING UNIT WITH 384 KBYTE WORKING MEMORY, 1. INTERFACE MPI/DP 12MBIT/S, 2. INTERFACE ETHERNET PROFINET, WITH 2 PORT SWITCH, MICRO MEMORY CARD NECESSARY",3465,"ST",1,"SIMATIC",0.46,1,"6AG13152EH147AB0"]
["6AG1315-2FJ14-2AB0","SIPLUS S7-300 CPU 315F-2PN/DP -25...+60Β°C with conformal coating based on 6ES7315-2FJ14-0AB0 . Central processing unit with 512 KB work memory, 1st interface MPI/DP 12Mbit/ s, 2nd interface Ethernet PROFINET, with 2-port switch, Micro Memory Card required",4190,"ST",1,"SIMATIC",0.52500000000000002,1,"6AG13152FJ142AB0"]
["6AG1315-6FF04-2AB0","SIPLUS S7-300 CPU 315F-2DP -25...+60Β°C with conformal coating based on 6ES7315-6FF04-0AB0 . Fail-safe module with MPI Integr. power supply 24 V DC, Work memory 384 KB, 40 mm width, 2nd interface DP master/ slave Micro Memory Card required",3014,"ST",1,"SIMATIC",0.36299999999999999,1,"6AG13156FF042AB0"]
["6AG1317-2EK14-7AB0","SIPLUS S7-300 CPU 317-2PN/DP -25...+70Β°C with conformal coating based on 6ES7317-2Ek14-0AB0 . Central processing unit with 1 MB work memory, 1st interface MPI/DP 12Mbit/ s, 2nd interface Ethernet PROFINET, with 2-port switch, Micro Memory Card required",6006,"ST",1,"SIMATIC",0.52,1,"6AG13172EK147AB0"]
["6AG1317-2FK14-2AB0","SIPLUS S7-300 CPU 317F-2PN/DP -25...+60Β°C with conformal coating based on 6ES7317-2FK14-0AB0 . Central processing unit with 1.5 MB work memory, 1st interface MPI/DP 12Mbit/ s, 2nd interface Ethernet PROFINET, with 2-port switch, Micro Memory Card required",6710,"ST",1,"SIMATIC",0.54300000000000004,1,"6AG13172FK142AB0"]
["6AG1317-6FF04-2AB0","SIPLUS S7-300 CPU 317F-2DP -25...+60Β°C with conformal coating based on 6ES7317-6FF04-0AB0 . Central processing unit with 1.5 MB work memory, 1st interface MPI/DP 12Mbit/ , 2nd interface DP master/ Slave, Micro Memory Card required Can be used with software package S7 Distributed Safety V5.2 SP1 or higher",6405,"ST",1,"SIMATIC",0.51800000000000002,1,"6AG13176FF042AB0"]
["6AG1321-1BH02-2AA0","SIPLUS S7-300 SM321 - 20-POLE -40 ... +70Β°C with conformal coating conformity with EN50155 T1 KAT 1 KL A/B based on 6ES7321-1BH02-0AA0. DIGITAL INPUT OPTIC. ISOLATED 16 DI, 24V DC, 1 X 20-POLE",321,"ST",1,"SIMATIC",0.22900000000000001,1,"6AG13211BH022AA0"]
["6AG1321-1BL00-2AA0","SIPLUS S7-300 SM321 - 40-POLE -40 ... +70Β°C with conformal coating conformity TO EN50155 T1 CAT 1 CL A/B based on 6ES7321-1BL00-0AA0. DIGITAL INPUT OPTICALLY ISOLATE 32DI, 24 V DC, 1 X 40 PIN",606,"ST",1,"SIMATIC",0.3,1,"6AG13211BL002AA0"]
["6AG1321-1CH20-2AA0","SIPLUS S7-300 SM 321 -25...+70 Β°C with conformal coating Conformity with EN 50155 T1 Kat 1 Kl A/B based on 6ES7321-1CH20-0AA0 . Digital input Isolated 16 DI, 48-125 V DC, 1x 20-pole",554,"ST",1,"SIMATIC",0.251,1,"6AG13211CH202AA0"]
["6AG1321-1FF01-2AA0","SIPLUS S7-300 SM 321-20-pole -40...+70Β°C with conformal coating Conformity with EN 50155 T1 Kat 1 Kl A/B based on 6ES7321-1FF01-0AA0 . Digital input Isolated 8 DI, 120 V/230 V AC",249,"ST",1,"SIMATIC",0.26,1,"6AG13211FF012AA0"]
["6AG1321-1FF10-7AA0","SIPLUS S7-300 SM321 8DI/120/230 -25...+70Β°C with conformal coating based on 6ES7321-1FF10-0AA0 . Digital input isolated, 8 DI, 120 V/230 V AC, 1x 40-pole, with single rooting/channel",440,"ST",1,"SIMATIC",0.33,1,"6AG13211FF107AA0"]
["6AG1321-1FH00-7AA0","SIPLUS S7-300 SM321 16DE/120/23 -40...+70Β°C with conformal coating based on 6ES7321-1FH00-0AA0 . Digital input isolated 16 DI, 120/230 V AC, 1x 20-pole",448,"ST",1,"SIMATIC",0.3,1,"6AG13211FH007AA0"]
["6AG1321-7BH01-2AB0","SIPLUS S7-300 SM 321-20-pole -25...+70Β°C with conformal coating Conformity with EN 50155 T1 Kat 1 Kl A/B based on 6ES7321-7BH01-0AB0. Digital \"input Isolated \"\"16 DI; 24 V DC,\" \"1x 20-pole,\"\" process interrupt,\" diagnostics, suitable for isochronous mode operation",606,"ST",1,"SIMATIC",0.23599999999999999,1,"6AG13217BH012AB0"]
["6AG1321-7BH01-4AS0","SIPLUS S7-300 SM 321 16DI 0-1 threshold at approx. 11.2 V with conformal coating based on 6ES7321-7BH01-0AB0 . Digital \"input SM 321, isolated, \"\"16 DI;\" \"24 V DC, 1x 20-pole,\"\" process\" interrupt, diagnostics, suitable for isochronous mode operation",745,"ST",1,"SIMATIC",0.246,1,"6AG13217BH014AS0"]
["6AG1321-7RD00-4AB0","SIPLUS S7-300 SM 321 4DI NAMUR for medial exposure with conformal coating based on 6ES7321-7RD00-0AB0 . Digital \"input Isolated \"\"4 DI; 24 V DC,\" NAMUR/DIN 19234, for signals from the hazardous area, diagnostics-capable, PTB tested",701,"ST",1,"SIMATIC",0.3,1,"6AG13217RD004AB0"]
["6AG1321-7TH00-4AB0","SIPLUS PCS 7 SM 321 16DI for medial exposure with conformal coating based on 6ES7321-7TH00-0AB0 . Digital \"input \"\"16 DI; 24 V DC, 1x\" \"40-pole,\"\" diagnostics-capable,\" for contacts (wired/ not wired), NAMUR encoder, 3/4-wire \"BERO, with chatter \"\"monitoring;\" \"Pulse\"\" extension, Open-circuit\" detection Connection IM 153-2 required",1355,"ST",1,"SIMATIC",0.38800000000000001,1,"6AG13217TH004AB0"]
["6AG1322-1BF01-2XB0","SIPLUS S7-300 SM 322 (-1BF01) -25...+70Β°C with conformal coating based on 6ES7322-1BF01-0AA0. Digital output SM 322, isolated, 8 DO, 24 V DC, 2A, 1x 20-pole",329,"ST",1,"SIMATIC",0.23,1,"6AG13221BF012XB0"]
["6AG1322-1BH01-2AA0","SIPLUS S7-300 SM322 - 20-POLE -25...+70Β°C with conformal coating with conformity EN50155 T1 CAT 1 KL A/B based on 6ES7322-1BH01-0AA0 . DIGITAL OUTPUT OPTIC. ISOLATED 16D0, 24V DC, 0.5A, SUM OF CURRENTS 4A/GROUP (8A/MODULE)",426,"ST",1,"SIMATIC",0.24,1,"6AG13221BH012AA0"]
["6AG1322-1BL00-2AA0","SIPLUS S7-300 SM322 32 DO - 40-POLE -25 ... +70Β°C with conformal coating conformity with EN50155 T1 KAT 1 KL A/B based on 6ES7322-1BL00-0AA0 . DIGITAL OUTPUT SM 322, OPTICALLY ISOLATED, 32DO, 24V DC, 0.5A, 1 X 40 PIN, SUM OF OUTPUT CURRENTS 4A/GROUP (16A/MODULE)",899,"ST",1,"SIMATIC",0.32,1,"6AG13221BL002AA0"]
["6AG1322-1CF00-7AA0","SIPLUS S7-300 SM 322 8DO 48-125V -25...+70Β°C with conformal coating based on 6ES7322-1CF00-0AA0 . Digital output isolated, 8 DO, 48-125 V DC, 1.5A, 1x 20-pole",731,"ST",1,"SIMATIC",0.31,1,"6AG13221CF007AA0"]
["6AG1322-1FF01-7AA0","SIPLUS S7-300 SM 322 8DO 120/ 220 -40...+70Β°C with conformal coating based on 6ES7322-1FF01-0AA0 . Digital output isolated, 8 DO, 120/230 V AC, 1 A, 1x 20-pole",499,"ST",1,"SIMATIC",0.307,1,"6AG13221FF017AA0"]
["6AG1322-1FH00-7AA0","SIPLUS S7-300 SM 322 16DO -40...+70Β°C with conformal coating based on 6ES7322-1FH00-0AA0 . Digital output Isolated 16 DO, 120/230 V AC, 1 A, 1x 20-pole",690,"ST",1,"SIMATIC",0.33900000000000002,1,"6AG13221FH007AA0"]
["6AG1322-1HF10-2AA0","SIPLUS S7-300 SM 322-40-pole -25...+60Β°C with conformal coating Conformity with EN 50155 T1 Cat 1 Cl A/B based on 6ES7322-1HF10-0AA0 . Digital output Isolated 8 DO (relay), 1x 40-pole, 24 V DC, 5 A or 230 V AC, 5 A, connectors with spring-loaded terminal can be used as of 6ES7392-1BM01-0AA0",383,"ST",1,"SIMATIC",0.29799999999999999,1,"6AG13221HF102AA0"]
["6AG1322-1HH01-2AA0","SIPLUS S7-300 SM 322-20-pole -40...+70Β°C with conformal coating Conformity with EN 50155 T1 Kat 1 Kl A/B based on 6ES7322-1HH01-0AA0 . Digital output optically isolated 16 DO, Relay contacts",626,"ST",1,"SIMATIC",0.3,1,"6AG13221HH012AA0"]
["6AG1322-5FF00-4AB0","SIPLUS S7-300 SM 322 8DO with conformal coating based on 6ES7322-5FF00-0AB0 . Digital output isolated, 8 DO, 120/230 V AC, 2A, with single rooting/channel and selectable failure mode, 1x 40-pole",593,"ST",1,"SIMATIC",0.33700000000000002,1,"6AG13225FF004AB0"]
["6AG1322-5HF00-4AB0","SIPLUS S7-300 SM 322 8RO 40pol with conformal coating based on 6ES7322-5HF00-0AB0 . Digital output isolated, 8 DO (relay), 1x 40-pole, 24 V DC, 120-230 V AC, 5 A with RC filter overvoltage protection",385,"ST",1,"SIMATIC",0.36,1,"6AG13225HF004AB0"]
["6AG1322-8BF00-2AB0","SIPLUS S7-300 SM 322-20-pole -25...+60Β°C EN 50155 conformity based on 6ES7322-8BF00-0AB0",703,"ST",1,"SIMATIC",0.3,1,"6AG13228BF002AB0"]
["6AG1322-8BH10-7AB0","SIPLUS S7-300 SM 322 16DO DC 24V -25...+70Β°C with conformal coating based on 6ES7322-8BH10-0AB0 . Digital \"output SM 322, \"\"16 DO; 24 V\" \"DC/0.5 A,\"\" diagnostics-capable,\" Wire break detection with 0 and 1 signal, 1x 40-pole, Connection IM 153-X HF required",1544,"ST",1,"SIMATIC",0.34300000000000003,1,"6AG13228BH107AB0"]
["6AG1323-1BH01-2AA0","SIPLUS S7-300 SM 323-20-pole -40...+70Β°C with conformal coating Conformity with EN 50155 T1 Kat 1 Kl A/B based on 6ES7323-1BH01-0AA0 . digital module Isolated 8DI and 8DO, 24 V DC, 0.5 A Total current 2 A",459,"ST",1,"SIMATIC",0.23699999999999999,1,"6AG13231BH012AA0"]
["6AG1326-1BK02-2AB0","SIPLUS S7-300 SM 326F DI24 40-pole -25...+60Β°C (70Β°C with forced convection) with conformal coating based on 6ES7326-1BK02-0AB0 . Digital input F-DI 24x24 V DC Fail-safe digital input for SIMATIC S7 F-systems with diagnostic alarm",2027,"ST",1,"SIMATIC",0.52,1,"6AG13261BK022AB0"]
["6AG1326-1RF01-4AB0","SIPLUS S7-300 SM 326F DI8 NAMUR for medial exposure with conformal coating based on 6ES7326-1RF01-0AB0 . Digital \"input \"\"SM 326, 8 DI; 24 V DC,\" \"NAMUR,\"\" fail-safe NAMUR input\" for SIMATIC S7 F-systems, up to Category 4 (EN 954-1)/ SIL3 (IEC 61508)/PLE (ISO 13849), 1x 40-pole",1659,"ST",1,"SIMATIC",0.56000000000000005,1,"6AG13261RF014AB0"]
["6AG1326-2BF10-2AB0","SIPLUS S7-300 SM 326 10F-DO -25...+60Β°C (70Β°C with forced convection) with conformal coating based on 6ES7326-2BF10-0AB0 . Digital output 24 V DC/2A PP, fail-safe digital output for SIMATIC S7F systems, with diagnostic alarm, LVV, 1x 40-pole",2205,"ST",1,"SIMATIC",0.52100000000000002,1,"6AG13262BF102AB0"]
["6AG1326-2BF41-2AB0","SIPLUS S7-300 SM 326F DO8 -25...+60Β°C with conformal coating based on 6ES7326-2BF41-0AB0 . Digital output F-DO 8x 24 V DC/2A PM fail-safe digital output Sinking-sourcing up to Category 4 (EN 954-1), SIL 3 (IEC 61508)",1607,"ST",1,"SIMATIC",0.48599999999999999,1,"6AG13262BF412AB0"]
["6AG1331-1KF02-7AB0","SIPLUS S7-300 SM331 8AE -25 ... +70Β°C with conformal coating based on 6ES7331-1KF02-0AB0 . OPTICALLY ISOLATED, 8 AI, 13 BIT RESOLUTION, U/I/RESISTANCE/PT100, NI100, NI1000, LG-NI1000, PTC / KTY, 66 MS MODULE UPDATE, 1 X 40 PIN",871,"ST",1,"SIMATIC",0.29399999999999998,1,"6AG13311KF027AB0"]
["6AG1331-6SB00-7AY0","SIPLUS LOGO! Power 24V 1,3A for medial stress -40...+70Β°C start up at -25Β°C based on 6EP3331-6SB00-0AY0 . stabilized power supply input: AC 100-240 V output: DC 24 V / 1,3 A",185,"ST",1,"LOGO!",0.14000000000000001,1,"6AG13316SB007AY0"]
["6AG1331-7KB02-2AB0","SIPLUS S7-300 SM 331-20-pole -25...+70Β°C with conformal coating based on 6ES7331-7KB02-0AB0 . Analog input isolated 2 AI, Resolution 9/12/14 bits, U/I/thermocouple/resistor, alarm, diagnostics, 1x 20-pole, Removing/inserting with active backplane bus",382,"ST",1,"SIMATIC",0.253,1,"6AG13317KB022AB0"]
["6AG1331-7KF02-2AB0","SIPLUS S7-300 SM331 20-POLE -25 ... +70Β°C with conformal coating conformity with EN50155 T1 KAT 1 KL A/B based on 6ES7331-7KF02-0AB0 . ANALOG INPUT GALVANICALLY ISOLATED 8 AI, AUFL. 9/12/14 BIT, U/I/THERMOEL./RESISTOR, ALARM, DIAGNOSTICS, 1 X 20-POLE, REMOVE/INSERT W.ACT. BACKPLANE BUS",1134,"ST",1,"SIMATIC",0.29199999999999998,1,"6AG13317KF022AB0"]
["6AG1331-7NF00-2AB0","SIPLUS S7-300 SM 331 40-pole -25...+70Β°C with conformal coating Conformity with EN 50155 T1 Kat 1 Kl A/B based on 6ES7331-7NF00-0AB0 . Analog \"input isolated \"\"8 AI; +/-5/10\" V, 1-5 V, +/-20 mA, 0/4 to 20 mA, 16 bit (55ms), Single rooting (50 V COM.)",1071,"ST",1,"SIMATIC",0.32200000000000001,1,"6AG13317NF002AB0"]
["6AG1331-7NF10-2AB0","SIPLUS S7-300 SM 331 8AI 40-pole -25...+60Β°C with conformal coating based on 6ES7331-7NF10-0AB0 . Analog \"input isolated, \"\"8 AI; +/-5/10\" V, 1-5 V, +/-20 mA, 0/4 to 20 mA, 16 bit, Single rooting (60 V COM.), 4-channel operation: 10 ms, 8-channel operation: 23-95ms, 1x 40-pole",1281,"ST",1,"SIMATIC",0.34,1,"6AG13317NF102AB0"]
["6AG1331-7PF01-4AB0","SIPLUS S7-300 SM 331 8AI with conformal coating based on 6ES7331-7PF01-0AB0 . Analog input isolated, 2/3/4-wire, 8 AI, Resistor, Pt100/200/1000 NI100/120/200/500/1000, CU10, characteristics according to GOST 16 (internal 24) bit, 50ms, 1x 40-pole",1628,"ST",1,"SIMATIC",0.33300000000000002,1,"6AG13317PF014AB0"]
["6AG1331-7PF11-4AB0","SIPLUS S7-300 SM 331 8AI 40-pole with conformal coating based on 6ES7331-7PF11-0AB0. Analog input isolated, 8 AI thermocouples Type B, E, J, K, L, N, R, S, T TXK/TXK (L) according to GOST 16 bit, 50ms, 1x 40-pole",1334,"ST",1,"SIMATIC",0.34,1,"6AG13317PF114AB0"]
["6AG1331-7RD00-2AB0","SIPLUS S7-300 SM 331 4AI -25...+60Β°C -25...+70Β°C (only 4-wire) with conformal coating based on 6ES7331-7RD00-0AB0",1250,"ST",1,"SIMATIC",0.36,1,"6AG13317RD002AB0"]
["6AG1331-7SF00-4AB0","SIPLUS S7-300 SM 331-20-pole medial exposure with conformal coating based on 6ES7331-7SF00-0AB0 without PTB approval",1229,"ST",1,"SIMATIC",0.25600000000000001,1,"6AG13317SF004AB0"]
["6AG1331-7TB00-7AB0","SIPLUS DP SM 331 2AE HART -25...+70 Β°C with conformal coating based on 6ES7331-7TB00-0AB0",1061,"ST",1,"SIMATIC",0.35499999999999998,1,"6AG13317TB007AB0"]
["6AG1331-7TF01-7AB0","SIPLUS SM 331 AI 8x0/4...20 mA -25...+70Β°C with conformal coating based on 6ES7331-7TF01-0AB0",1617,"ST",1,"SIMATIC",0.25,1,"6AG13317TF017AB0"]
["6AG1332-1SH71-4AA0","SIPLUS S7-1200 PM 1207 for medial exposure with conformal coating based on 6EP1332-1SH71 . Stabilized power supplies Input: 120/230 V AC Output: 24 V DC/2.5 A",147,"ST",1,"SIMATIC",0.3,1,"6AG13321SH714AA0"]
["6AG1332-1SH71-7AA0","SIPLUS S7-1200 PM 1207 -25...+70 Β°C with conformal coating based on 6EP1332-1SH71 . Stabilized power supplies Input: 120/230 V AC output: 24 V DC/2.5 A",173,"ST",1,"SIMATIC",0.3,1,"6AG13321SH717AA0"]
["6AG1332-4BA00-7AA0","SIPLUS S7-1500 PM 1507 24 V/3 A -40 ... +70Β°C with conformal coating based on 6EP1332-4BA00 . STABILIZED POWER SUPPLY INPUT: 120/230 V AC OUTPUT: 24 V/3 A DC",333,"ST",1,"SIMATIC",0.45,1,"6AG13324BA007AA0"]
["6AG1332-5HB01-2AB0","SIPLUS S7-300 SM 332-20-pole -25...+70Β°C with conformal coating Conformity with EN 50155 T1 Kat 1 Kl A/B based on 6ES7332-5HB01-0AB0 . Analog \"output isolated, \"\"2 AI, U/I;\" Resolution 11/12 bit 20-pole, Removing/inserting with active backplane bus possible",650,"ST",1,"SIMATIC",0.23799999999999999,1,"6AG13325HB012AB0"]
["6AG1332-5HD01-7AB0","SIPLUS S7-300 SM 332 4AO U/I -25...+70Β°C with conformal coating based on 6ES7332-5HD01-0AB0 . Analog \"output SM 332, isolated, \"\"4 AO,\" \"U/I; diagnostics;\"\" resolution\" 11/12 bits, 20-pole, removing and inserting possible with active backplane bus",1026,"ST",1,"SIMATIC",0.251,1,"6AG13325HD017AB0"]
["6AG1332-5HF00-2AB0","SIPLUS S7-300 SM332 40POLE -25...+70Β°C with conformal coating based on 6ES7332-5HF00-0AB0 . ANALOG OUTPUT OPTICALLY ISOLATED, 8 \"AO, U/I; DIAGNOSTICS;\" RESOLUTION 11/12 BITS, 40 PIN, REMOVE/INSERT W. ACTIVE, BACKPLANE BUS",1806,"ST",1,"SIMATIC",0.30499999999999999,1,"6AG13325HF002AB0"]
["6AG1332-6SB00-7AY0","SIPLUS LOGO! Power 24V 2,5A for medial stress -40...+70Β°C start up at -25Β°C based on 6EP3332-6SB00-0AY0 . stabilized power supply input: AC 100-240 V output: DC 24 V / 1,3 A",195,"ST",1,"LOGO!",0.23,1,"6AG13326SB007AY0"]
["6AG1332-7ND02-4AB0","SIPLUS S7-300 SM 332 4AO with conformal coating based on 6ES7332-7ND02-0AB0 . Analog output isolated by channel, 4 AI, Resolution 16 bit, 0-10 V, 1-5 V, +/-10 V, +/-20 mA, 0/4-20mA, 20-pole, suitable for isochronous mode operation improved bus cycle times for+ the isochronous mode",1176,"ST",1,"SIMATIC",0.29499999999999998,1,"6AG13327ND024AB0"]
["6AG1332-8TF01-2AB0","SIPLUS S7-300 SM 332 8AO HART -25...+60Β°C with conformal coating based on 6ES7332-8TF01-0AB0 . Analog output 8 AO 0/4-20 mA HART, for ET 200M with IM 153-2, IM 153-2, 20-pole Functions: FW update, HART auxiliary variables, redundancy, local diagnostic buffer with time stamping, Requirement: PCS 7 V7.0, SP1",2111,"ST",1,"SIMATIC",0.26,1,"6AG13328TF012AB0"]
["6AG1333-3BA10-7AA0","SIPLUS PS PSU200M 5A with conformal coating based on 6EP1333-3BA10 . STABILIZED Power-Supply Input: 120/230-500V AC Output: 24 V/5 A DC",447,"ST",1,"SIMATIC",0.6,1,"6AG13333BA107AA0"]
["6AG1333-4BA00-7AA0","SIPLUS S7-1500 PM 1507 24 V/8 A -40 ... +70Β°C with conformal coating based on 6EP1333-4BA00 . STABILIZED POWER SUPPLY FOR SIMATIC S7-1500 INPUT: 120/230 V AC OUTPUT: 24 V/8 A DC",418,"ST",1,"SIMATIC",0.73599999999999999,1,"6AG13334BA007AA0"]
["6AG1333-6SB00-7AY0","SIPLUS LOGO! Power 24V 4A for medial stress -40...+70Β°C start up at -25Β°C based on 6EP3333-6SB00-0AY0 . stabilized power supply input: 100-240 V AC output: 24 V / 1.3 A DC",237,"ST",1,"LOGO!",0.3,1,"6AG13336SB007AY0"]
["6AG1334-0KE00-7AB0","SIPLUS S7-300 SM 334 4AI 2AO -25...+70Β°C with conformal coating based on 6ES7334-0KE00-0ab0 . Analog module isolated, 4 AI/2 AO, 12 bit, 0-10 V for Pt100 (climatic range -120-155Β°C) and 10 kOhm measuring range, 1x 20-pole",869,"ST",1,"SIMATIC",0.24,1,"6AG13340KE007AB0"]
["6AG1334-2BA20-4AA0","SIPLUS PSU100S 24 V/10 A FOR medial stress based on 6EP1334-2BA20 . STABILIZED POWER SUPPLY INPUT: OUTPUT: 24 V/10 A DC",412,"ST",1,"SIMATIC",0.7,1,"6AG13342BA204AA0"]
["6AG1334-3BA10-7AA0","SIPLUS PS PSU200M 10 A -25...+70Β°C with conformal coating based on 6EP1334-3BA10 . STABILIZED Power-Supply Input: 120/230-500V AC Output: 24 V/10 A DC",514,"ST",1,"SIMATIC",0.8,1,"6AG13343BA107AA0"]
["6AG1336-4GE00-2AB0","SIPLUS S7-300 SM336 F 6AI 15 bit -25...+60 Β°C (70 Β°C with forced convection) With conformal coating Based on 6ES7336-4GE00-0AB0 . Fail-safe analog inputs For SIMATIC Safety, with HART support, up to Category 4 (EN 954-1) /SIL3 (IEC 61508)/ PLE (ISO 13849), 1x 20-pole",1817,"ST",1,"SIMATIC",0.34,1,"6AG13364GE002AB0"]
["6AG1337-8SB00-7AY0","SIPLUS PS PSU8200 40A -40 Β°C...+70Β°C with conformal coating based on 6EP3337-8SB00-0AY0 . Stabilized power supply Input: 120/230 C AC Output: 24 V DC/40 A",1155,"ST",1,"SIMATIC",3,1,"6AG13378SB007AY0"]
["6AG1340-1AH02-2AE0","SIPLUS S7-300 CP 340 RS232 -25...+70Β°C based on 6ES7340-1AH02-0AE0 . Communications processor with RS232C interface (RS-232-C) incl. configuration package auf CD-ROM",944,"ST",1,"SIMATIC",0.36,1,"6AG13401AH022AE0"]
["6AG1340-1CH02-2AE0","SIPLUS S7-300 CP 340 RS422/485 -25...+60Β°C conformal coating based on 6ES7340-1CH02-0AE0. Communications processor with RS 422/485 interface incl. configuration package auf CD-ROM",1071,"ST",1,"SIMATIC",0.36,1,"6AG13401CH022AE0"]
["6AG1341-1AH02-7AE0","SIPLUS S7-300, CP 341 -25...+70 Β°C with conformal coating based on 6ES7341-1AH02-0AE0 . Communications processor with RS232C interface (RS-232-C) incl. configuration package auf CD-ROM",1743,"ST",1,"SIMATIC",0.30399999999999999,1,"6AG13411AH027AE0"]
["6AG1341-1CH02-7AE0","SIPLUS S7-300 CP 341 RS422/485 -25...+70Β°C with conformal coating based on 6ES7341-1CH02-0AE0",1680,"ST",1,"SIMATIC",0.30399999999999999,1,"6AG13411CH027AE0"]
["6AG1342-5DA03-7XE0","SIPLUS NET CP 342-5 PROFIBUS -25...+70Β°C based on 6GK7342-5DA03-0XE0 . Communications processor CP 342-5 for connecting SIMATIC S7-300 to PROFIBUS, DP, S5-compatible, PG/OP and S7 communication",1817,"ST",1,"SIMATIC",0.3,1,"6AG13425DA037XE0"]
["6AG1343-1CX10-2XE0","SIPLUS NET CP 343-1 Lean -25...+60Β°C with conformal coating based on 6GK7343-1CX10-0XE0 . Communications processor for connection of SIMATIC S7-300 to Ind. Ethernet via TCP/IP and UDP, MULTICAST, Send/Receive with and without RFC1006, fetch/ write, S7 communication (server) PROFINET IO device integrated 2-port switch ERTEC 200, Size exchange without PG, SNMP diagnostics, Initialization via LAN, 2x RJ45 connection for LAN with 10/100 Mbit/s",1502,"ST",1,"SIMATIC",0.26600000000000001,1,"6AG13431CX102XE0"]
["6AG1343-1EX30-7XE0","SIPLUS NET CP 343-1 -25...+70 Β°C with conformal coating based on 6GK7343-1EX30-0XE0 . Communications processor for connection of SIMATIC S7-300 to Industrial Ethernet via ISO and TCP/IP, PROFINET IO controller or PROFINET IO device, Integrated 2-port switch ERTEC 200, S7 communication, fetch/write, Send/Receive with and without RFC1006, MULTICAST DHCP, NTC-CPU Sync, diagnostics, initialization via LAN, 2x RJ45 connection for LAN with 10/100 Mbit/s",2520,"ST",1,"SIMATIC",0.28699999999999998,1,"6AG13431EX307XE0"]
["6AG1343-1GX31-4XE0","SIPLUS NET CP 343-1 Advanced with conformal coating based on 6GK7343-1GX31-0XE0 . for connection of the SIMATIC \"S7-300 CPU to Ind. Ethernet;\" PROFINET IO controller and/or \"IO Device; RT and RT and IRT\" \"IRT, MRP, PROFINET CBA; TCP/IP\" ISO, UDP, S7 COM, S5-comp. com., (send/receive) with Fetch/Write with and without RFC 1006, MULTICAST Diagnostic extension,SNMP,DHCP, FTP client/server, e-mail, Gigabit-SS1X RJ45 (10/100/1000) PROFINET-SS 2x RJ45(10/100 \"Mbit) \"\"PROFINET CBA; security\"\"\" \"(firewall/VPN); PROFIenergy\"",3066,"ST",1,"SIMATIC",0.50600000000000001,1,"6AG13431GX314XE0"]
["6AG1344-0SB00-7AY0","SIPLUS PS PSU100E 48V/5A -40...+70Β°C start up -25Β°C with conformal coating based on 6EP3344-0SB00-0AY0 . Stabilized power supply Input: 120 / 230 V AC Output: 48 V/5 A DC",630,"ST",1,"SIMATIC",0.5,1,"6AG13440SB007AY0"]
["6AG1350-1AH03-2AE0","SIPLUS S7-300 FM350-1 -25...+60 Β°C with conformal coating based on 6ES7350-1AH03-0AE0. Counter module Counter functions up to 500 kHz 1 channel for connection of 5 V and 24 V incremental encoders \"Isochronous mode; Measuring\" range types incl. configuration package auf CD-ROM",831,"ST",1,"SIMATIC",0.28000000000000003,1,"6AG13501AH032AE0"]
["6AG1350-2AH01-4AE0","SIPLUS S7-300 FM350-2 8 channels for medial exposure with conformal coating based on 6ES7350-2AH01-0AE0 . Counter module FM 350-2, 8 channels, 20 kHz, 24 V encoder for counting, frequency measurement, speed measurement, period duration measurement, dosing incl. configuration package and Electronic documentation on CD-ROM",2100,"ST",1,"SIMATIC",0.47299999999999998,1,"6AG13502AH014AE0"]
["6AG1365-0BA01-2AA0","SIPLUS S7-300 IM 365 -25...+60 Β°C EN 50155 conformity based on 6ES7365-0BA01-0AA0 . Connection IM 365 for connection of an extension rack without C bus, 2 modules+ connecting cable 1 m",307,"ST",1,"SIMATIC",0.61299999999999999,1,"6AG13650BA012AA0"]
["6AG1370-0AA01-7AA0","SIPLUS S7-300 DM370 -40...+70 Β°C with conformal coating based on 6ES7370-0AA01-0AA0. Dummy module Use for module replacement",305,"ST",1,"SIMATIC",0.22,1,"6AG13700AA017AA0"]
["6AG1400-1JA11-7AA0","SIPLUS S7-400 rack UR2 9-slot Alu -25...+70Β°C with conformal coating based on 6ES7400-1JA11-0AA0 . central and distributed 2 redundant PS can be plugged in",1407,"ST",1,"SIMATIC",1.8180000000000001,1,"6AG14001JA117AA0"]
["6AG1400-1TA11-7AA0","SIPLUS S7-400 rack UR1 18-slot Al -25...+70Β°C with conformal coating based on 6ES7400-1TA11-0AA0 . central and distributed with 18 slots, 2 redundant PS can be plugged in",2226,"ST",1,"SIMATIC",4,1,"6AG14001TA117AA0"]
["6AG1400-2JA10-7AA0","SIPLUS S7-400 rack UR2-H -25...+70Β°C with conformal coating based on 6ES7400-2JA10-0AA0 . central and distributed with 2x 9 slots",2342,"ST",1,"SIMATIC",3.2829999999999999,1,"6AG14002JA107AA0"]
["6AG1405-0KA02-7AA0","SIPLUS S7-400 PS 405 10 A -25...+70Β°C with conformal coating based on 6ES7405-0KA02-0AA0 . Power \"supply, Wide range \"\"10 A,\" \"24/48/60 V DC; 5 V DC/10 A\"\"\"",1491,"ST",1,"SIMATIC",1.2789999999999999,1,"6AG14050KA027AA0"]
["6AG1405-0KR02-7AA0","SIPLUS S7-400 PS 405 10 A -25...+70Β°C with conformal coating based on 6ES7405-0KR02-0AA0. 10A, Wide \"range, \"\"24/48/60 V DC; 5 V\" \"DC/10 A,\"\" for redundant use\"",1880,"ST",1,"SIMATIC",1.353,1,"6AG14050KR027AA0"]
["6AG1407-0KA02-7AA0","SIPLUS S7-400 PS 407 10 A -25...+70Β°C with conformal coating based on 6ES7407-0KA02-0AA0 . 10A, Wide \"range, \"\"UC 120/230V; 5 V DC/10\" \"A\"\"\"",1596,"ST",1,"SIMATIC",1.2709999999999999,1,"6AG14070KA027AA0"]
["6AG1407-0KR02-7AA0","SIPLUS S7-400 PS 407 10 A -25...+70Β°C with conformal coating based on 6ES7407-0KR02-0AA0 . 10A, Wide \"range, \"\"UC 120/230V; 5 V DC/10\" \"A,\"\" for redundant use\"",1859,"ST",1,"SIMATIC",1.2829999999999999,1,"6AG14070KR027AA0"]
["6AG1410-5AA00-4FW6","SIPLUS IPC 277E 7\" TOUCH - Flottweg LO 0β€¦+55Β°C with Conformal Coating based on 6AV7410-5AA00-1FW6 . Bundle, with customer-specific Express design and WinCC RT PRO 512, SIMATIC WinCC Recipes, for Flottweg SE",8085,"ST",1,"SIMATIC",1.5,1,"6AG14105AA004FW6"]
["6AG1410-5HX08-7AB0","SIPLUS PCS 7 CPU 410-5H -25...+70Β°C with conformal coating based on 6ES7410-5HX08-0AB0 . Central processing unit for S7-400 and S7-400H/F/FH, 5 interfaces: 1x PN, 1x DP, 2x for Sync modules \"and 1x service . \"\"Only for\" \"spare parts supply;\"\" without\" System Expansion Card",17115,"ST",1,"SIMATIC",0.85,1,"6AG14105HX087AB0"]
["6AG1411-5AB10-2AA0","SIPLUS NET IE/PB LINK PN IO -40...+60Β°C start up -40Β°C with conformal coating based on 6GK1411-5AB10 . IE/PB Link PN IO Gateway between Ind.ETHERNET and PROFIBUS with PROFINET IO functionality S7 routing and data record routing, 10/100 MBit fast ETHERNET, MRP, 9.6 KBit/s up to 12 MBit PROFIBUS, NTP.",2678,"ST",1,"SIMATIC",0.48199999999999998,1,"6AG14115AB102AA0"]
["6AG1412-5AA00-4FW6","SIPLUS IPC 277E 12\" TOUCH - Flottweg LO 0β€¦+55Β°C with Conformal Coating based on 6AV7412-5AA00-1FW6 . SIPLUS IPC277E, 12\" Touch Bundle, with customer-specific Express design and WinCC RT PRO 512, SIMATIC WinCC Recipes, for Flottweg SE",9030,"ST",1,"SIMATIC",2.75,1,"6AG14125AA004FW6"]
["6AG1412-5HK06-7AB0","SIPLUS S7-400 CPU 412-5H -25...+70Β°C with conformal coating based on 6ES7412-5HK06-0AB0 . Central processing unit for S7-400H and S7-400F/FH, 5 interfaces: 1x MPI/DP, 1x DP, 1x PN and 2 for SYNC modules, 1 MB memory (512 KB data/512 KB program)",6090,"ST",1,"SIMATIC",1.1559999999999999,1,"6AG14125HK067AB0"]
["6AG1414-3EM07-7AB0","SIPLUS S7-400 CPU 414-3 PN/DP -25 ... +70Β°C with conformal coating based on 6ES7414-3EM07-0AB0 . Central processing unit with: Work memory 4 MB, (2 MB code, 2 MB data), Interfaces 1st interface MPI/DP 12 Mbit/s, (X1), 2nd interface ETHERNET/PROFINET (X5) 3rd interface IF 964-DP plug-in (IF1)",8999,"ST",1,"SIMATIC",0.83599999999999997,1,"6AG14143EM077AB0"]
["6AG1414-5HM06-7AB0","SIPLUS S7-400 CPU 414-5H -25...+70Β°C with conformal coating based on 6ES7414-5HM06-0AB0 . Central processing unit for S7-400H and S7-400F/FH, 5 interfaces: 1x MPI/DP, 1x DP, 1x PN and 2 for SYNC modules, 4 MB memory (512 KB data/512 KB program)",11760,"ST",1,"SIMATIC",1.1559999999999999,1,"6AG14145HM067AB0"]
["6AG1416-3ES07-7AB0","SIPLUS S7-400 CPU 416-3 PN/DP -25 ... +70Β°C with conformal coating based on 6ES7416-3ES07-0AB0 . Central processing unit with: Work memory 16 MB, (8 MB code, 8 MB data), Interfaces 1st interface MPI/DP 12 Mbit/s, (X1), 2nd interface ETHERNET/PROFINET (X5) 3rd interface IF 964-DP plug-in (IF1)",16800,"ST",1,"SIMATIC",1.0089999999999999,1,"6AG14163ES077AB0"]
["6AG1416-3XS07-7AB0","SIPLUS S7-400 CPU 416-3 -25... +70Β°C with conformal coating based on 6ES7416-3XS07-0AB0. Central processing unit with: Work memory 16 MB, (8 MB code, 8 MB data), Interfaces 1st interface MPI/DP 12 Mbit/s, 2nd interface PROFIBUS DP, 3rd interface plug-in IFM module",16380,"ST",1,"SIMATIC",0.83599999999999997,1,"6AG14163XS077AB0"]
["6AG1416-5HS06-7AB0","SIPLUS S7-400 CPU 416-5H -25...+70Β°C with conformal coating based on 6ES7416-5HS06-0AB0 . Central processing unit for S7-400H and S7-400F/FH, 5 interfaces: 1x MPI/DP, 1x DP, 1x PN and 2 for SYNC modules, 16 MB memory (512 KB data/512 KB program)",17115,"ST",1,"SIMATIC",1.1559999999999999,1,"6AG14165HS067AB0"]
["6AG1417-4XT07-7AB0","SIPLUS S7-400 CPU 417-4 -25 ... +70Β°C with conformal coating based on 6ES7417-4XT07-0AB0. Central processing unit with: \"Work memory 32 MB, (16 MB code;\" 16 MB data) Interfaces 1st \"interface MPI 12 Mbit/s; 2nd\" interface PROFIBUS DP, 3rd/4th interface plug-in IFM module",19005,"ST",1,"SIMATIC",1.004,1,"6AG14174XT077AB0"]
["6AG1417-5HT06-7AB0","SIPLUS S7-400 CPU 417-5H -25...+70Β°C with conformal coating based on 6ES7417-5HT06-0AB0 . Central processing unit for S7-400H, and S7-400F/FH 5 interfaces: 1x MPI/DP, 1x DP, 1x PN and 2 for SYNC modules, 32 MB memory (16 MB data/16 MB program)",22260,"ST",1,"SIMATIC",1.1559999999999999,1,"6AG14175HT067AB0"]
["6AG1421-1BL01-2AA0","SIPLUS S7-400 SM 421 32DI -25...+60Β°C based on 6ES7421-1BL01-0AA0",572,"ST",1,"SIMATIC",0.75700000000000001,1,"6AG14211BL012AA0"]
["6AG1422-1BL00-2AA0","SIPLUS S7-400 SM 422 32DO -25...+60Β°C based on 6ES7422-1BL00-0AA0",777,"ST",1,"SIMATIC",0.75900000000000001,1,"6AG14221BL002AA0"]
["6AG1431-0HH00-4AB0","SIPLUS S7-400 SM 431 16AI for medial exposure based on 6ES7431-0HH00-0AB0",1481,"ST",1,"SIMATIC",0.8,1,"6AG14310HH004AB0"]
["6AG1432-1HF00-4AB0","SIPLUS S7-400 SM 432 8AO for medial exposure based on 6ES7432-1HF00-0AB0",1691,"ST",1,"SIMATIC",0.76400000000000001,1,"6AG14321HF004AB0"]
["6AG1433-2BA20-7AA0","SIPLUS PS PSU300S 5A -25 ... +70Β°C with conformal coating based on 6EP1433-2BA20. STABILIZED POWER SUPPLY INPUT: 3 400-500 V 3AC OUTPUT: 24 V DC/5 A",380,"ST",1,"SIMATIC",0.5,1,"6AG14332BA207AA0"]
["6AG1434-2BA20-7AA0","SIPLUS PS PSU300S 10A -25 ... +70Β°C with conformal coating based on 6EP1434-2BA20. STABILIZED POWER SUPPLY INPUT: 400-500 V 3AC OUTPUT: 24 V DC/10 A",422,"ST",1,"SIMATIC",0.7,1,"6AG14342BA207AA0"]
["6AG1435-2AD00-4AA0","SIPLUS D435-2 DP/PN 0...+55Β°C with conformal coating based on 6AU1435-2AD00-0AA0 . SIPLUS \"Drive-based Control \"\"Unit\" \"D435-2 DP/PN;\"\" Programmable\" \"Motion Control controller;\" \"Standard performance;\" Interfaces: 12 DI, 16 DI/DO, 6 DRIVE-CLiQ, 2 PROFIBUS, 3 PROFINET ports, 2 Ethernet, 2 \"USB, \"\"1 option slot; incl.\"\"\" Double fan/battery module and battery",4851,"ST",1,"SIMATIC",4.5,1,"6AG14352AD004AA0"]
["6AG1436-2BA10-7AA0","SIPLUS PS PSU300S 20 A for medial exposure -40Β°C...+70Β°C based on 6EP1436-2BA10. Stabilized power supplies Input: 3 AC 400-500V Output: DC 24V/20A",453,"ST",1,"SIMATIC",1.6,1,"6AG14362BA107AA0"]
["6AG1437-3BA10-7AA0","SIPLUS PSU8200 3-ph. 24 V DC 40 A -25...+70Β°C with conformal coating based on 6EP1437-3BA10 . Stabilized power supplies Input: 400-500V 3 AC Output: 24 V DC/40 A",761,"ST",1,"SIMATIC",3.4,1,"6AG14373BA107AA0"]
["6AG1443-1EX30-4XE0","SIPLUS NET CP 443-1 for medial exposure with conformal coating based on 6GK7443-1EX30-0XE0. \"2x 10/100 Mbit/s (IE switch);\" \"RJ45 ports; \"\"ISO; TCP; UDP;\" \"PROFINET IO CON \"\"TROLLER; S7\" \"communication;\"\" open\" communication (SEND/RE- \"CEIVE); S7 routing; IP\" configu- ration via \"DHCP/block;\"\"via \"\"IP Access\" \"Control List; Clock-\"\" \"\"Time\" \"synchronization; extended \"\"Web\" \"diagnostics; fast start up ;\"\"\" Support for PROFIenergy",3329,"ST",1,"SIMATIC",0.82099999999999995,1,"6AG14431EX304XE0"]
["6AG1443-1GX30-4XE0","SIPLUS NET CP 443-1 Advanced for medial exposure with conformal coating based on \"6GK7443-1GX30-0XE0 . \"\"1x\" \"10/100/1000 Mbit/s;\"\" \"\"4x 10/100\" \"Mbit/s (IE switch);\"\" \"\"RJ45\" \"ports;\"\" \"\"ISO; TCP; UDP;\" \"PROFINET IO CON \"\"TROLLER; S7\" \"communication;\"\" open\" communication (SEND/RE- \"CEIVE); S7 routing; IP\" configu- ration via \"DHCP/block;\"\"via \"\"IP Access\" \"Control List; Clock-\"\" \"\"Time\" \"synchronization; extended \"\"Web\" \"diagnostics; fast start up;\"\"\" \"PROFIenergy support; \"\"IP\" \"routing; FTP; Web server;\"\"\" E-mail PROFINET C(*)",4337,"ST",1,"SIMATIC",0.84499999999999997,1,"6AG14431GX304XE0"]
["6AG1443-5DX05-4XE0","SIPLUS NET CP 443-5 for medial exposure based on 6GK7443-5DX05-0XE0 . Communications processor extended for connection of SIMATIC S7-400 on PROFIBUS, DP, S5-compatible PG/OP and S7 communication",2867,"ST",1,"SIMATIC",0.8,1,"6AG14435DX054XE0"]
["6AG1443-5FX02-4XE0","SIPLUS NET CP 443-5 Basic for medial exposure with conformal coating based on 6GK7443-5FX02-0XE0 . Communications processor for connection of SIMATIC S7-400 on PROFIBUS, FMS, S5-compatible PG/OP and S7 communication",2898,"ST",1,"SIMATIC",0.8,1,"6AG14435FX024XE0"]
["6AG1455-2AD00-4AA0","SIPLUS D455-2 DP/PN 0...+55Β°C with conformal coating based on 6AU1455-2AD00-0AA0 . SIPLUS \"Drive-based \"\"Control Unit\" \"D455-2 DP/PN;\"\" \"\"Programmable\" \"motion controller \"\"ULTRA-High\" \"Performance;\"\" Interfaces: 12\" DI, 16 DI/DO, 6 DRIVE-CLiQ, 2 PROFIBUS, 3 PROFINET ports, 2 \"Ethernet, 2 USB, \"\"1 option\" \"slot;\"\" incl. dual fan/ battery\" module and battery",9692,"ST",1,"SIMATIC",5,1,"6AG14552AD004AA0"]
["6AG1460-0AA01-2AB0","SIPLUS S7-400 IM 460-0 TX for -25...+60Β°C based on 6ES7460-0AA01-0AB0",786,"ST",1,"SIMATIC",0.82,1,"6AG14600AA012AB0"]
["6AG1461-0AA01-2AA0","SIPLUS S7-400 IM 461-0 RX for -25...+60Β°C based on 6ES7461-0AA01-0AA0",755,"ST",1,"SIMATIC",0.82299999999999995,1,"6AG14610AA012AA0"]
["6AG1500-0EA02-2AA0","SIPLUS NET PB Connector for -25...+60Β°C and MED based on 6GK1500-0EA02",112,"ST",1,"SIMATIC",0.104,1,"6AG15000EA022AA0"]
["6AG1503-2CA01-2AA0","SIPLUS NET OLM/P11 V4.0 -25...+60Β°C start up temperature:-25Β°C with conformal coating based on 6GK1503-2CA01 . optical link module with 1 RS485 and 1 Plastic FOC interface (2 BFOC sockets), with signaling contact and test port",735,"ST",1,"SIMATIC",0.5,1,"6AG15032CA012AA0"]
["6AG1503-2CB00-2AA0","SIPLUS NET OLM/G11 V4.0 -25...+60Β°C based on 6GK1503-2CB00",995,"ST",1,"SIMATIC",0.5,1,"6AG15032CB002AA0"]
["6AG1503-2CC00-2AA0","SIPLUS NET OLM/G11-1300 V4.0 -25...+60Β°C with conformal coating based on 6GK1503-2CC00 . Optical Link Module with 1 RS485 and 1 glass FOC interface (2 BFOC sockets), 1300Nm Shaft Length for large distances with signaling contact and test port",2447,"ST",1,"SIMATIC",0.5,1,"6AG15032CC002AA0"]
["6AG1503-3CA01-2AA0","SIPLUS NET OLM/P12 V4.1 -25...+60Β°C start up temperature: -25Β°C with conformal coating based on 6GK1503-3CA01 . optical link module with 1 RS485 and 1 Plastic FOC interface (2 BFOC sockets), with signaling contact and test port",885,"ST",1,"SIMATIC",0.5,1,"6AG15033CA012AA0"]
["6AG1503-3CB00-2AA0","SIPLUS NET OLM/G12 V4.0 -25...+60Β°C based on 6GK1503-3CB00",1439,"ST",1,"SIMATIC",0.5,1,"6AG15033CB002AA0"]
["6AG1503-3CC00-2AA0","SIPLUS NET OLM G12-1300 V4.0 -25β€¦+60Β°C with conformal coating based on 6GK1503-3CC00 . PROFIBUS OLM/G12-1300 V4.0 Optical Link Module with 1 RS-485 and 2 glas-LWL- interfaces (4 BFOC- Buchsen), 1300Nm wave-length for large distances with signal contact and test port.",4074,"ST",1,"SIMATIC",0.42699999999999999,1,"6AG15033CC002AA0"]
["6AG1503-3CC00-4AA0","SIPLUS NET OLM/G12-1300 V4.0 for medial exposure based on 6GK1503-3CC00",3129,"ST",1,"SIMATIC",0.5,1,"6AG15033CC004AA0"]
["6AG1505-0KA00-7AB0","SIPLUS S7-1500 PS 1505 25W 24VD 40...+70Β°C start up -25Β°C with conformal coating based on 6ES7505-0KA00-0AB0 . SYSTEM POWER SUPPLY SUPPLIES THE OPERATING VOLTAGE THE S7-1500 VIA THE BACKPLANE B",344,"ST",1,"SIMATIC",0.35,1,"6AG15050KA007AB0"]
["6AG1505-0RA00-7AB0","SIPLUS S7-1500, System power supply PS 60W 24/48/60 V DC, supplies the backplane bus of the S7-1500 with operating voltage -25...+70Β°C with conformal coating based on 6ES7505-0RA00-0AB0",854,"ST",1,"SIMATIC",0.5,1,"6AG15050RA007AB0"]
["6AG1507-0RA00-7AB0","SIPLUS S7-1500, System power supply PS 60W 120/AC 230 V DC, supplies the backplane bus of the S7-1500 with operating voltage -40...+70Β°C start up -25Β°C with conformal coating based on 6ES7507-0RA00-0AB0",855,"ST",1,"SIMATIC",0.5,1,"6AG15070RA007AB0"]
["6AG1510-1DJ01-2AB0","SIPLUS ET 200SP CPU 1510SP-1 PN -40...+60Β°C with conformal coating based on 6ES7510-1DJ01-0AB0 . CPU 1510SP-1 PN for ET 200SP, Central processing unit with Work memory 100 KB for program and 750 KB for data, first interface: PROFINET IRT with 3-port switch, 72 ns bit performance, SIMATIC Memory Card required, BusAdapter required",1155,"ST",1,"SIMATIC",0.5,1,"6AG15101DJ012AB0"]
["6AG1510-1DJ01-7AB0","SIPLUS ET 200SP CPU 1510SP-1 PN -40...+70 Β°C With conformal coating based on 6ES7510-1DJ01-0AB0 . Central processing unit with 100 KB work memory for program and 750 KB for data, 1st interface: PROFINET IRT with 3-port switch, 72 ns bit performance, SIMATIC memory card required, BusAdapter required for port 1 and 2",1460,"ST",1,"SIMATIC",0.40400000000000003,1,"6AG15101DJ017AB0"]
["6AG1510-1SJ01-2AB0","SIPLUS ET 200SP CPU 1510SP F-1PN -25...+60Β°C start up -25 Β°C with conformal coating based on 6ES7510-1SJ01-0AB0. Central processing unit with Work memory 150 KB for program and 750 KB for data, 1st interface: PROFINET IRT with 3-port switch, 72 ns bit performance, SIMATIC Memory Card required, Bus Adapter required for Port 1 and 2",1596,"ST",1,"SIMATIC",0.5,1,"6AG15101SJ012AB0"]
["6AG1511-1AK02-2AB0","SIPLUS S7-1500 CPU 1511-1 PN -40Β°CΒ…+60Β°C with conformal coating based on 6ES7511-1AK02-0AB0 . Central processing unit with Work memory 150 KB for program and 1 MB for data, 1st interface: PROFINET IRT with 2-port switch, 60 ns bit performance, SIMATIC Memory Card required",1134,"ST",1,"SIMATIC",0.50700000000000001,1,"6AG15111AK022AB0"]
["6AG1511-1AK02-7AB0","SIPLUS S7-1500 -40β€¦+70Β°C with conformal coating based on 6ES7511-1AK02-0AB0 . SIMATIC S7-1500, CPU 1511-1 PN, Zentralbaugruppe mit Arbeitsspeicher 150 KB fΓΌr Programm u: 1MByte fΓΌr Daten 1. Schnittstelle: PROFINET IRT mit 2 Port Switch, 60 NS Bit-Performance, SIMATIC MemoryCard notwendig",2090,"ST",1,"SIMATIC",0.50700000000000001,1,"6AG15111AK027AB0"]
["6AG1512-1DK01-2AB0","SIPLUS ET 200SP CPU 1512SP-1 PN -40...+60Β°C with conformal coating based on 6ES7512-1DK01-0AB0 . CPU 1512SP-1 PN for ET 200SP, Central processing unit with Work memory 200 KB for program and 1 MB for data, first interface: PROFINET IRT with 3-port switch, 48 ns bit performance, SIMATIC Memory Card required, BusAdapter required for port 1 and 2",1481,"ST",1,"SIMATIC",0.5,1,"6AG15121DK012AB0"]
["6AG1512-1DK01-7AB0","SIPLUS ET 200SP CPU 1512SP-1 PN -40...+70 Β°C With conformal coating based on 6ES7512-1DK01-0AB0 . Central processing unit with 200 KB work memory for program and 1 MB for data, 1st interface: PROFINET IRT with 3-port switch, 48 ns bit performance, SIMATIC memory card required, BusAdapter required for port 1 and 2",1775,"ST",1,"SIMATIC",0.5,1,"6AG15121DK017AB0"]
["6AG1512-1SK01-2AB0","SIPLUS ET 200SP CPU 1512SP F-1P -25...+60Β°C start up -25Β°C with conformal coating based on 6ES7512-1SK01-0AB0 . Central processing unit with RAM 300 KB for program and 1 MB for data, 1st interface: PROFINET IRT with 3-port switch, 48 ns bit performance, SIMATIC Memory Card required, Bus Adapter required for Port 1 and 2",2079,"ST",1,"SIMATIC",0.41499999999999998,1,"6AG15121SK012AB0"]
["6AG1513-1AL01-7AB0","SIPLUS S7-1500 CPU 1513-1 PN -40...+70Β°C start up -20Β°C with conformal coating based on 6ES7513-1AL01-0AB0 . Central processing unit with Work memory 300 KB for program and 1.5 MB for data, 1st interface: PROFINET IRT with 2-port switch, 40 ns bit performance, SIMATIC Memory Card required",3119,"ST",1,"SIMATIC",0.504,1,"6AG15131AL017AB0"]
["6AG1513-1AL02-2AB0","SIPLUS S7-1500 CPU 1513-1 PN -40Β°CΒ…+60Β°C with conformal coating based on 6ES7513-1AL02-0AB0 . Central processing unit with Work memory 300 KB for program and 1.5 MB for data, 1st interface: PROFINET IRT with 2-port switch, 40 ns bit performance, SIMATIC Memory Card required",2520,"ST",1,"SIMATIC",0.504,1,"6AG15131AL022AB0"]
["6AG1513-1AL02-7AB0","SIPLUS S7-1500 CPU 1513-1 PN -40...+70Β°C with Conformal Coating based on 6ES7513-1AL02-0AB0 . central processing unit with working memory 300 KB for program and 1.5 MB for data, 1. interface: PROFINET IRT with 2 port switch, 40 NS bit-performance, SIMATIC memory card necessary",3140,"ST",1,"SIMATIC",0.504,1,"6AG15131AL027AB0"]
["6AG1515-2FM01-2AB0","SIPLUS S7-1500 CPU 1515F-2 PN -25Β°C to 60Β°C with conformal coating based on 6ES7515-2FM01-0AB0. central processing unit with working memory 750 KB for program and 3 MB for data, 1. Interface: PROFINET IRT WITH 2 PORT SWITCH, 2. Interface: PROFINET RT, 30 NS BIT-PERFORMANCE,SIMATIC MEMORY CARD NECESSARY",4809,"ST",1,"SIMATIC",0.91600000000000004,1,"6AG15152FM012AB0"]
["6AG1515-2RM00-7AB0","SIPLUS S7-1500 CPU 1515R-2 PN -40...+70Β°C with Conformal Coating based on 6ES7515-2RM00-0AB0 . central processing unit with working memory 500 KB for program and 3 MB data, 1. interface: PROFINET RT with 2 port switch, 2. interface PROFINET RT, SIMATIC memory card necessary",5555,"ST",1,"SIMATIC",0.91500000000000004,1,"6AG15152RM007AB0"]
["6AG1516-3AN01-2AB0","SIPLUS S7-1500 CPU 1516-3 PN/DP -40 ... +60Β°C start up -20 Β°C with conformal coating based based on 6ES7516-3AN01-0AB0. CENTRAL PROCESSING UNIT WITH WORKING MEMORY 1 MB FOR PROGRAM AND 5 MB FOR DATA, 1. INTERFACE: PROFINET IRT WITH 2 PORT SWITCH, 2. INTERFACE: ETHERNET, 3. INTERFACE: PROFIBUS, 10 NS BIT-PERFORMANCE, SIMATIC MEMORY CARD NECESSARY",6447,"ST",1,"SIMATIC",0.94,1,"6AG15163AN012AB0"]
["6AG1516-3AN01-7AB0","SIPLUS S7-1500 CPU 1516-3 PN/DP -40...+70Β°C start up -20Β°C with conformal coating based on 6ES7516-3AN01-0AB0 . Central processing unit with Work memory 150 KB for program and 1 MB for data, 1st interface: PROFINET IRT with 2-port switch, 60 ns bit performance, SIMATIC Memory Card required",6741,"ST",1,"SIMATIC",0.94,1,"6AG15163AN017AB0"]
["6AG1516-3FN01-2AB0","SIPLUS S7-1500 CPU-1516F-3 PN/DP -25...+60Β°C start up -20 Β°C with conformal coating based on 6ES7516-3FN01-0AB0. Central processing unit with RAM 1.5 MB for program and 5 MB for data, 1st interface: PROFINET IRT with 2-port switch, 2nd interface: Ethernet, 3rd interface: PROFIBUS, 10 ns bit performance, SIMATIC Memory Card required",7665,"ST",1,"SIMATIC",0.93600000000000005,1,"6AG15163FN012AB0"]
["6AG1518-4AP00-4AB0","SIPLUS S7-1500 CPU 1518-4 PN/DP with conformal coating based on 6ES7518-4AP00-0AB0 . Central processing unit with Work memory 3 MB for Program and 10 MB for data, 1st interface, PROFINET IRT with 2-port switch, 2nd interface, Ethernet, 3rd interface, Ethernet, 4th interface, PROFIBUS, 1 ns bit-performance, SIMATIC Memory Card required",12390,"ST",1,"SIMATIC",0.6,1,"6AG15184AP004AB0"]
["6AG1518-4AX00-4AC0","SIPLUS S7-1500 CPU 1518-4 PN/DP MFP with conformal coating based on 6ES7518-4AX00-1AC0. inklusive C/C++ Runtime und OPC UA Runtime Lizenz Arbeits- speicher 4 MByte fΓΌr Programm und 20MByte fΓΌr Daten, 1. Schnittstelle: PROFINET IRT mit 2 Port Switch, 2. Schnitt- stelle: PROFINET RT, 3. Schnitt- stelle: Ethernet, 4. Schnitt- stelle: PROFIBUS, 1 NS Bit- Performance, SIMATIC Memory Card (min. 2 GB) notwendig",13440,"ST",1,"SIMATIC",2.1349999999999998,1,"6AG15184AX004AC0"]
["6AG1518-4FP00-4AB0","SIPLUS S7-1500 CPU 1518F-4 PN/DP with conformal coating based on 6ES7518-4FP00-0AB0. Central processing unit with Work memory 4.5 MB for program and 10 MB for data, 1st interface, PROFINET IRT with 2-port switch 2nd interface, Ethernet, 3rd interface, Ethernet, 4th interface, PROFIBUS, 1 ns bit-performance, SIMATIC Memory Card required",14805,"ST",1,"SIMATIC",2.1440000000000001,1,"6AG15184FP004AB0"]
["6AG1521-1BH00-7AB0","SIPLUS S7-1500 DI 16x24 V DC HF -40...+70Β°C with conformal coating based on 6ES7521-1BH00-0AB0 . Digital \"input module \"\"16 channels in\" \"groups of 16;\"\" \"\"Input delay\" \"0.05..20ms \"\"Input type 3 (IEC\" \"61131);\"\" \"\"diagnostics; hardware\" \"interrupts\"\"\"",333,"ST",1,"SIMATIC",0.27100000000000002,1,"6AG15211BH007AB0"]
["6AG1521-1BH50-7AA0","SIPLUS S7-1500 DI 16x24 V DC SRC -40...+70Β°C with conformal coating based on 6ES7521-1BH50-0AA0 . Digital \"input module \"\"DI 16x24 V DC,\" \"source-input;\"\" \"\"16 channels in\" \"groups of 16;\"\" \"\"Input delay 3.2\" \"ms;\"\" Input type 3 (IEC 61131)\"",266,"ST",1,"SIMATIC",0.2,1,"6AG15211BH507AA0"]
["6AG1521-1BL00-7AB0","SIPLUS S7-1500 DI 32X24VDC HF -40 ... +70Β°C with conformal coating based on. Digital input module DI 32x24V DC HF, 32 channels in groups of 16 Input delay 0.05..20 ms Input type 3 (IEC 61131) diagnostics Hardware interrupts",521,"ST",1,"SIMATIC",0.2,1,"6AG15211BL007AB0"]
["6AG1521-1FH00-7AA0","SIPLUS S7-1500 DI 16x230V AC BA -40...+70Β°C with conformal coating based on 6ES7521-1FH00-0AA0 . Digital input module DI 16x230 V AC, \"16 channels in groups of 4;\" \"Input delay 20ms; Input type\" 1 (IEC 61131)",372,"ST",1,"SIMATIC",0.2,1,"6AG15211FH007AA0"]
["6AG1521-7EH00-7AB0","SIPLUS S7-1500 DI 16x 48VUC/ 125V -40...+70Β°C with conformal coating based on \"6ES7521-7EH00-0AB0 . \"\"16\" \"channels in groups of 1;\"\"\" Input delay 0.05..20ms Input \"type 3 (IEC 61131);\"\"\" \"diagnostics; hardware\" \"interrupts\"\"\"",911,"ST",1,"SIMATIC",0.27100000000000002,1,"6AG15217EH007AB0"]
["6AG1522-1BF00-7AB0","SIPLUS S7-1500 DQ 8x24 V DC/2A -40...+70Β°C with conformal coating based on 6ES7522-1BF00-0AB0 . Digital \"output module \"\"DQ 8x24 V DC/2A\" \"HF;\"\" \"\"8 channels in groups of\" \"8;\"\" \"\"8 A per group;\"\"\" \"diagnostics; substitute value\"",302,"ST",1,"SIMATIC",0.2,1,"6AG15221BF007AB0"]
["6AG1522-1BH01-7AB0","SIPLUS S7-1500 DQ 16X24VDC/0.5A -40 ... +70Β°C MIT conformal coating based on 6ES7522-1BH01-0AB0 . 16 CHANNELS IN GROUPS OF 8, 4 A \"PER GROUP; SINGLE-CHANNEL\" \"DIAGNOSIS; SUBSTITUTE VALUE\"",418,"ST",1,"SIMATIC",0.29099999999999998,1,"6AG15221BH017AB0"]
["6AG1522-1BL01-7AB0","SIPLUS S7-1500 DQ 32x24VDC/0.5A -40 ... +70Β°C with conformal coating based on 6ES7522-1BL01-0AB0 . 32 CHANNELS IN GROUPS OF 8, 4 A \"PER GROUP; SINGLE-CHANNEL\" \"DIAGNOSIS; SUBSTITUTE VALUE\"",729,"ST",1,"SIMATIC",0.33900000000000002,1,"6AG15221BL017AB0"]
["6AG1522-5EH00-7AB0","SIPLUS S7-1500 DQ 16x48VUC/125V -40...+70Β°C with conformal coating based on \"6ES7522-5EH00-0AB0 . \"\"DQ16x\" \"24...48VUC/125V DC/0.5A; \"\"16\" \"channels in groups of 1;\"\" \"\"0.5\" \"A per group;\"\" Substitute\" \"value;\"\" Observe derating\"",1407,"ST",1,"SIMATIC",0.2,1,"6AG15225EH007AB0"]
["6AG1522-5FF00-7AB0","SIPLUS S7-1500 DO 8x230V AC/2A -40...+70Β°C with conformal coating based on 6ES7522-5FF00-0AB0 . Digital \"output module \"\"DQ 8xAC 230V/2A;\" \"TRIAC;\"\" \"\"8 channels in groups\" \"of 1;\"\" \"\"2 A per group;\"\"\" Substitute value",371,"ST",1,"SIMATIC",0.2,1,"6AG15225FF007AB0"]
["6AG1522-5FH00-7AB0","SIPLUS S7-1500 16DQ 230VAC 1A ST TRIAC -40 ... +70Β°C start up -25Β°C with conformal coating based on 6ES7522-5FH00-0AB0 . SIMATIC S7-1500, Digital output module \"DQ 16xAC 230V/1A; TRIAC; 16\" \"channels in groups of 2; 2 A\" \"per group; Substitute value\"",727,"ST",1,"SIMATIC",0.2,1,"6AG15225FH007AB0"]
["6AG1522-5HF00-2AB0","SIPLUS S7-1500 DQ 8X230VAC/5A S -25 ... +60Β°C with conformal coating based on 6ES7522-5HF00-0AB0 . DIGITAL OUTPUT MODULE DQ 8 X \"230VAC/5A,RELAY; 8 CHANNELS IN\" \"GROUPS OF 1, 5A PER GROUP;\" \"DIAGNOSIS; SUBSTITUTE VALUE\"",554,"ST",1,"SIMATIC",0.2,1,"6AG15225HF002AB0"]
["6AG1522-5HH00-7AB0","SIPLUS S7-1500 16DQ 230VAC 2A RLY -40 ... +70Β°C start up -25 Β°C with conformal coating based on 6ES7522-5HH00-0AB0. Digital output module DQ 16 X \"230VAC / 2A ST; RELAY; 16\" channels in groups of 2, 4A per \"group; Diagnosois;\"",705,"ST",1,"SIMATIC",0.2,1,"6AG15225HH007AB0"]
["6AG1526-1BH00-2AB0","SIPLUS S7-1500 F-DI 16x24VDC -25 ... +60Β°C with conformal coating based on 6ES7526-1BH00-0AB0 . FAILSAFE DIGITAL INPUT MODULE, F-DI \"16X24VDC PROFISAFE; 35 MM\" \"WIDTH; UP TO PL E (ISO\" 13849-1)/ SIL3 (IEC 61508)",1197,"ST",1,"SIMATIC",0.09,1,"6AG15261BH002AB0"]
["6AG1526-2BF00-2AB0","SIPLUS S7-1500 F-DQ 8x24VDC/2A -25 ... +60Β°C with conformal coating based on 6ES7526-2BF00-0AB0 . F DIGITAL OUTPUT MODULE, F-DQ 8X24VDC 2A \"PPM PROFISAFE; 35 mm overall\" \"width; UP TO PL E (ISO\" 13849-1)/ SIL3 (IEC 61508)",1365,"ST",1,"SIMATIC",0.09,1,"6AG15262BF002AB0"]
["6AG1531-7KF00-7AB0","SIPLUS S7-1500 AI 8xU/I/RTD/TC -40Β°C ... +70Β°C with conformal coating based on 6ES7531-7KF00-0AB0 . Analog input module 16 bit resolution, Accuracy 0.3%, 8 channels in \"groups of 8, \"\"Common mode\" \"voltage 10 V;\"\" \"\"diagnostics;\" \"hardware interrupts\"\" incl.\" infeed element, Shield bracket and shield terminal",1003,"ST",1,"SIMATIC",0.2,1,"6AG15317KF007AB0"]
["6AG1531-7NF00-7AB0","SIPLUS S7-1500 AI 8XU/I HF -40 ... +70Β°C with conformal coating based on 6ES7531-7NF00-0AB0 . 16 bit resolution, Accuracy 0.1%, 8 channels in groups of 1, Common mode voltage: 30V AC/60V DC, \"diagnostics; hardware\" \"interrupts; incl. infeed\" element, Shield bracket and shield terminal",1365,"ST",1,"SIMATIC",0.3,1,"6AG15317NF007AB0"]
["6AG1531-7NF10-7AB0","SIPLUS S7-1500 AI 8xU/I HS -40 Β°C ... +70Β°C with conformal coating based on 6ES7531-7NF10-0AB0 . Analog input module AI 8xU/I HS, 16 bit resolution, Accuracy 0.4% 8 channels in groups of 8, \"Common mode voltage 10 V;\" \"diagnostics; hardware\" \"interrupts\"\" 8 channels in 0.125\" ms incl. infeed element, Shield bracket and shield terminal",1218,"ST",1,"SIMATIC",0.2,1,"6AG15317NF107AB0"]
["6AG1531-7PF00-4AB0","SIPLUS S7-1500 AI 8XU/R/RTD/TC HF 0 ... +60Β°C with conformal coating based on 6ES7531-7PF00-0AB0 . Analog Input Module AI 8 X U/R/RTD/TC HF, 16 BITS OF RESOLUTION, Accuracy 0.1%, 8 Channels in \"groups of 1; common mode\" Voltage: 30 V AC/60 V DC, \"Diagnosis, Process alarms;\" incl. infeed element, Shield clamp and Shield terminal",1533,"ST",1,"SIMATIC",0.3,1,"6AG15317PF004AB0"]
["6AG1532-5HD00-7AB0","SIPLUS S7-1500 AO 4xU/I ST -40 Β°C ... +70Β°C with conformal coating based on 6ES7532-5HD00-0AB0 . Analog output module 16 bit resolution, Accuracy 0.3%. 4 channels in groups of 4, \"diagnostics; substitute value\" incl. infeed element, shield bracket and shield terminal",854,"ST",1,"SIMATIC",0.2,1,"6AG15325HD007AB0"]
["6AG1532-5HF00-7AB0","SIPLUS S7-1500 AQ 8xU/I HS -40...+70 Β°C Start up -25 Β°C with conformal coating based on 6ES7532-5HF00-0AB0 . Analog output module AQ8xU/I HS, 16 bit resolution, Accuracy 0.4%, 8 channels in groups of 8, \"diagnostics; substitute value\" 8 channels in 0.125 ms incl. infeed element, Shield bracket and shield terminal",1218,"ST",1,"SIMATIC",0.2,1,"6AG15325HF007AB0"]
["6AG1540-1AB00-7AA0","SIPLUS S7-1500CM PtP RS422/485 -40...+70Β°C start up -25Β°C with conformal coating based on 6ES7540-1AB00-0AA0 . Communication module for Serial connection RS422, RS485 Freeport, 3964 (R), USS, 19200 Kbit/s, 15-Pin D-sub socket",920,"ST",1,"SIMATIC",0.2,1,"6AG15401AB007AA0"]
["6AG1540-1AD00-7AA0","SIPLUS S7-1500cm PtP RS232 BA -40...+70Β°C start up -25Β°C with conformal coating based on 6ES7540-1AD00-0AA0 . Communication module for Serial connection RS232, Freeport, 3964 (R), USS, 19200 Kbit/s, 9-pin D-sub connector",693,"ST",1,"SIMATIC",0.5,1,"6AG15401AD007AA0"]
["6AG1541-1AB00-7AB0","SIPLUS S7-1500CM PtP RS422/485 -40...+70Β°C start up -25Β°C with conformal coating based on 6ES7541-1AB00-0AB0 . Communication module for Serial connection RS422 and RS485, Freeport, 3964 (R), USS, MODBUS RTU Master, Slave, 115200 Kbit/s, 15-Pin D-sub socket",1502,"ST",1,"SIMATIC",0.5,1,"6AG15411AB007AB0"]
["6AG1541-1AD00-7AB0","SIPLUS S7-1500 CM PtP RS232 HF -40...+70Β°C start up -25Β°C with conformal coating based on 6ES7541-1AD00-0AB0 . Communication module for Serial connection RS232, Freeport, 3964 (R), USS, MODBUS RTU Master, Slave, 115200 Kbit/s, 9-pin D-sub connector",1407,"ST",1,"SIMATIC",0.5,1,"6AG15411AD007AB0"]
["6AG1542-5DX00-7XE0","SIPLUS NET CM 1542-5 (Profibus -40...+70Β°C with conformal coating based on 6GK7542-5DX00-0XE0 . Communication module for connection of S7-1500 to PROFIBUS DP as DP master and DP slave: S7 and PG/OP communication, time-of-day synchronization, Diagnostics",1523,"ST",1,"SIMATIC",0.2,1,"6AG15425DX007XE0"]
["6AG1543-1AX00-2XE0","SIPLUS CP 1543-1 -40...+60Β°C start up -25Β°C with conformal coating based on 6GK7543-1AX00-0XE0 Communications processor for connecting SIMATIC S7-1500 to Industrial Ethernet: TCP/IP, ISO, UDP, S7 communication, IP-BROADCAST/ MULTICAST, security (hardware identification, IP/MAC access list, firewall), Diagnostics SNMPV1/V3, DHCP, FTP client/ server, Email, IPV4/IPV6, data storage on SD Card of the CPU, time-of-day synchronization via \"NTP, Access to the \"\"Web server\" \"of the CPU; Gigabit interface\"\"\" 1x RJ45 (10/100/1000 MB)",2772,"ST",1,"SIMATIC",0.1,1,"6AG15431AX002XE0"]
["6AG1543-1MX00-7XE0","SIPLUS TIM 1531 IRC -40...+70Β°C with conformal coating based on 6GK7543-1MX00-0XE0 . communication module for SIMATIC S7-1500, S7-400, S7-300 with SINAUT ST7 with three RJ145 interfaces for communication via IP-based networks (WAN / LAN) and a RS-232/RS-485- Interface for Communications via classic WAN networks",4095,"ST",1,"SIMATIC",0.35599999999999998,1,"6AG15431MX007XE0"]
["6AG1545-5DA00-2AB0","SIPLUS ET 200SP CM DP -40...+60Β°C with conformal coating based on 6ES7545-5DA00-0AB0 . CM PROFIBUS DP for ET 200SP CPU Module w. PROFIBUS DP interface (9-pole D-sub socket) DP master for 125 DP slaves",784,"ST",1,"SIMATIC",0.104,1,"6AG15455DA002AB0"]
["6AG1550-1AA00-7AB0","SIPLUS S7-1500 TM Count 2x24V -40...+70Β°C with conformal coating based on 6ES7550-1AA00-0AB0 . Counter module, 2 channels for 24 V incremental or encoder 3 DI, 2 DQ per channel",836,"ST",1,"SIMATIC",0.5,1,"6AG15501AA007AB0"]
["6AG1551-1AB00-7AB0","SIPLUS S7-1500 TM POSINPUT 2 -40...+70Β°C start up -25Β°C with conformal coating based on 6ES7551-1AB00-0AB0 . Counting and position feedback module, 2 channels, for RS422 incremental encoder or SSI absolute value encoder, 2 DI, 2 DQ per channel",923,"ST",1,"SIMATIC",0.5,1,"6AG15511AB007AB0"]
["6AG1590-0AA00-7AA0","SIPLUS S7-1500 U-connector -25...+70Β°C with conformal coating based on 6ES7590-0AA00-0AA0 . Spare part \"for the \"\"connection of I/O\" \"modules;\"\" Self-assembling\" backplane bus 5 units per packing unit",292,"PAK",1,"SIMATIC",0.05,1,"6AG15900AA007AA0"]
["6AG1591-1AA01-2AA0","SIPLUS S7-1500 front flap V2 CPU 35 mm -25...+60Β°C start up -20Β°C with conformal coating based on 6ES7591-1AA01-0AA0 . Display for CPU 1511-1 PN, CPU 1511F-1 PN, CPU 1511C-1 PN, CPU 1512C-1 PN, CPU 1513-1 PN and CPU 1513F-1 PN",240,"ST",1,"SIMATIC",8.7999999999999995E-2,1,"6AG15911AA012AA0"]
["6AG1591-1BA01-2AA0","SIPLUS S7-1500 front flap V2 CPU 70 mm -25...+60Β°C start up -20Β°C with conformal coating based on 6ES7591-1BA01-0AA0 . SIMATIC S7-1500, Spare part Display for CPU 1515 (F)-2 PN, CPU 1516 (F)-3 PN/DP, CPU 1517 (F)-3 PN/DP and CPU 1518 (F)-4 PN/DP",240,"ST",1,"SIMATIC",0.14799999999999999,1,"6AG15911BA012AA0"]
["6AG1592-6EF00-2AA0","SIPLUS S7-1500 E-CODING ELEMENTS TYPE F spare part -25 ... +60Β°C with conformal coating based on 6ES7592-6EF00-1AA0 . 5 E-CODING ELEMENTS TYPE F FOR ET 200MP \"MODULE F-DI, F-DQ; 5 UNITS PER\" PACKING UNIT",166,"ST",1,"SIMATIC",8.9999999999999993E-3,1,"6AG15926EF002AA0"]
["6AG1620-0AA00-7AA0","SIPLUS PN/CAN LINK -40Β°C - 70 Β°C with conformal coating based on 6BK1620-0AA00-0AA0. from Profinet to CAN or CANopen networks CAN 2.0A/B CANopen Manager to CiA301/302 CANopen Slave to CiA301/302 IP20",830,"ST",1,"SIMATIC",0.21199999999999999,1,"6AG16200AA007AA0"]
["6AG1647-0AH11-2AX0","SIPLUS HMI KP300 Basic mono PN -25...+60Β°C with conformal coating based on 6AV6647-0AH11-3AX0",445,"ST",1,"SIMATIC",0.32,1,"6AG16470AH112AX0"]
["6AG1654-5CJ00-7XF0","SIPLUS PCS 7 CPU 410-5H Bundle PO 100 -25...+70Β°C with conformal coating based on 6ES7654-5CJ00-0XF0 . PROCESS Automation for S7-400 and S7-400H/F/HF with system expansion card up to 100 process objects",17325,"ST",1,"SIMATIC",1.5,1,"6AG16545CJ007XF0"]
["6AG1654-5CL00-7XF0","SIPLUS PCS 7 CPU 410-5H bundle -25...+70Β°C with conformal coating based on 6ES7654-5CL00-0XF0 . Process Automation for S7-400 and S7-400H with system expansion card up to 500 process objects",19635,"ST",1,"SIMATIC",1.5,1,"6AG16545CL007XF0"]
["6AG1654-5CN00-7XF0","SIPLUS PCS 7 CPU 410-5H bundle -25...+70Β°C with conformal coating based on 6ES7654-5CN00-0XF0 . Process Automation for S7-400 and S7-400H with system expansion card up to 1000 process objects",22680,"ST",1,"SIMATIC",1.5,1,"6AG16545CN007XF0"]
["6AG1654-5CP00-7XF0","SIPLUS PCS 7 CPU 410-5H bundle -25...+70Β°C with conformal coating based on 6ES7654-5CP00-0XF0 . Process Automation for S7-400 and S7-400H with system expansion card up to 1600 process objects",26250,"ST",1,"SIMATIC",1.5,1,"6AG16545CP007XF0"]
["6AG1654-5CQ00-7XF0","SIPLUS PCS 7 CPU 410-5H bundle -25Β°C...+70Β°C with conformal coating based on 6ES7654-5CQ00-0XF0 . Process Automation for S7-400 and S7-400H with system expansion card more than 2000 process objects",32130,"ST",1,"SIMATIC",1.5,1,"6AG16545CQ007XF0"]
["6AG1654-7HY00-7XA0","SIPLUS S7 bus module for Y couplers -25...+70Β°C based on 6ES7654-7HY00-0XA0",130,"ST",1,"SIMATIC",0.247,1,"6AG16547HY007XA0"]
["6AG1677-2DB42-2GB0","SIPLUS ET 200SP CPU1515SP PC2 -40...+60Β°C with Conformal Coating based on 6ES7677-2DB42-0GB0 . 8 GB RAM, 30 GB CFast with Windows 10 IoT Enterprise 64 bit and S7-1500 Software Controller CPU 1505SP pre-installed, Interfaces: 1x slot CFast, 1x slot SD/MMC, 1x connection for ET 200SP bus adapter PROFINET, 1x 10/100/1000 Mbit/s Ethernet 2x USB 3.0; 2x USB 2.0, 1x display port, documentation on USB stick, restore USB stick",3728,"ST",1,"SIMATIC",0.83,1,"6AG16772DB422GB0"]
["6AG1677-2SB42-2GB0","SIPLUS ET 200SP CPU1515SP PC2 F -40...+60Β°C with Conformal Coating based on 6ES7677-2DB42-0GB0 . 8 GB RAM, 30 GB CFast with Windows 10 IoT Enterprise 64 bit and S7-1500 Failsafe Software Controller CPU 1505SP F pre-installed, Interfaces: 1x slot CFast, 1x slot SD/MMC, 1x connection for ET 200SP bus adapter PROFINET, 2x USB 3.0; 2x USB 2.0, 1x display port, documentation on USB stick, restore USB stick 1x 10/100/1000 Mbit/s Ethernet",4305,"ST",1,"SIMATIC",0.83,1,"6AG16772SB422GB0"]
["6AG1688-3AF37-2AX0","SIPLUS HMI KP8F PN -20β€¦+55Β°C with Conformal Coating based on 6AV3688-3AF37-0AX0 . Key Panel, 8 short-stroke switches with multi-colored LEDs, PROFINET interfaces with PROFIsafe; 8 DI/DO and 2 safety DI pins, 24 V DC can be looped through parameterizable as of STEP 7 V5.5",861,"ST",1,"SIMATIC",0.35599999999999998,1,"6AG16883AF372AX0"]
["6AG1688-3AY36-2AX0","SIPLUS HMI KP8 PN -25...+60Β°C with conformal coating based on 6AV3688-3AY36-0AX0",601,"ST",1,"SIMATIC",0.32900000000000001,1,"6AG16883AY362AX0"]
["6AG1688-3EH47-2AX0","SIPLUS HMI KP32F PN -20β€¦+55Β°C with Conformal Coating based on 6AV3688-3EH47-0AX0 . Key Panel, 32 short-stroke keys with multi-colored LEDs, PROFINET interfaces with PROFIsafe, 16 DI+16 DI/DO, 4 safety DI pins, 24 V DC can be looped through parameterizable as of STEP 7 V5.5",2436,"ST",1,"SIMATIC",1.907,1,"6AG16883EH472AX0"]
["6AG1688-3XY38-2AX0","SIPLUS HMI Design empty front in KP8 format -25...+60Β°C With conformal coating based on 6AV3688-3XY38-3AX0 . Design empty front in KP8 format for easy mounting of standard 22.5 mm operator controls ideal for the setup of modular operator panels Also suitable for installation in extension units of the pro devices",225,"ST",1,"SIMATIC",0.30599999999999999,1,"6AG16883XY382AX0"]
["6AG1720-3AA01-7XX0","SIPLUS ST7 MD720 2G -40...+70 Β°C start up -25Β°C with conformal coating based on 6NH9720-3AA01-0XX0 . GSM/GPRS, 2G mobile radio modem with \"RS232 interface; for GSM\" \"services CSD, GPRS, \"\"SMS;\" \"Quadband GSM;\"\" \"\"AT command\" \"interface;\"\" observe national\" \"approvals! \"\"autom. GPRS\" \"connection setup; incl. gender\" changer for RS232/PPI adapter",873,"ST",1,"SIMATIC",0.11,1,"6AG17203AA017XX0"]
["6AG1732-0AA00-7AA0","SIPLUS PS DC/DC 24 V/2 A 0Β°C...70Β°C with conformal coating based on 6EP1732-0AA00 . SITOP POWER 2 A, DC/DC STABILIZED POWER SUPPLIES INPUT: DC 48/60/110 V Output: 24 V DC/2 A",453,"ST",1,"SIMATIC",0.5,1,"6AG17320AA007AA0"]
["6AG1800-3BA00-7AA0","SIPLUS ST7 TIM 3V-IE -25...+70 Β°C with conformal coating based on 6NH7800-3BA00 . communication module for \"SIMATIC S7-300 and C7; with\" one RS232 interface for SINAUT communication via classic WAN and an RJ45 interface for SINAUT communication via an IP-based network (WAN or LAN)",1764,"ST",1,"SIMATIC",0.315,1,"6AG18003BA007AA0"]
["6AG1800-4BA00-7AA0","SIPLUS ST7 TIM 4R-IE -25...+70 Β°C with conformal coating based on 6NH7800-4BA00 . communication module for SIMATIC S7-300, S7-400, C7, PC with two RS232/RS485 interfaces for SINAUT Communications via classic WANs and two RJ45 interfaces for SINAUT communication via IP-based networks (WAN or LAN)",4536,"ST",1,"SIMATIC",0.48099999999999998,1,"6AG18004BA007AA0"]
["6AG1803-3BA00-7AA0","SIPLUS NET TIM 3V-IE DNP3 for medial exposure -25...+70Β°C based on 6NH7803-3BA00-0AA0 communication module for SIMATIC S7-300 with an RS232 interface",1764,"ST",1,"SIMATIC",0.315,1,"6AG18033BA007AA0"]
["6AG1803-4BA00-7AA0","SIPLUS NET TIM 4R-IE DNP3 -25...+70Β°C with conformal coating based on 6NH7803-4BA00-0AA0. TIM 4R-IE DNP3 communication module for \"SIMATIC S7-300, \"\"S7-400, PC;\" \"with two\"\" RS232/RS485\" interfaces for DNP3 communication via classic WANs and two RJ45 interfaces for DNP3 communication via IP- based networks (WAN or LAN)",4683,"ST",1,"SIMATIC",0.47199999999999998,1,"6AG18034BA007AA0"]
["6AG1900-0AB00-7AA0","SIPLUS NET C-Plug -40...+70Β°C with conformal coating based on 6GK1900-0AB00 . removable data storage medium for simple Replacement of devices in case of failure for recording configuration or project engineering and application data, Can be used in SIMATIC NET products with C-Plug slot",61.4,"ST",1,"SIMATIC",0.03,1,"6AG19000AB007AA0"]
["6AG1900-0AB01-4AA0","SIPLUS C-Plug 256 0β€¦+60Β°C with conformal coating based on 6GK1900-0AB01 . C-plug 256 (CP 343-1 Advanced) removable data storage medium for simple Replacement of the devices in case of fault or failure; for holding configuration or planning and application data, 256 MB, Can only be used in CP 343-1 Advanced",336,"ST",1,"SIMATIC",2.7E-2,1,"6AG19000AB014AA0"]
["6AG1900-0AB10-7AA0","SIPLUS C-Plug -40β€¦+70Β°C with conformal coating based on 6GK1900-0AB10 . removable data storage medium for simple device replacement in case of fault, for recording configuration or configuration and application data, can be used in the following SIMATIC NET products with C-plug slot, SCALANCE XC-200, XP-200, XM-400, XR-500, M-800 S615 and W-700",242,"ST",1,"SIMATIC",2.7E-2,1,"6AG19000AB107AA0"]
["6AG1901-1BB10-7AA0","SIPLUS NET RJ45 plug 180 2x2 -40...+70Β°C with conformal coating based on 6GK1901-1BB10-2AA0 . RJ45 plug-in connector (10/100 Mbit/s) with rugged Metal enclosure and FC connection Technology, for IE FC Cable 2x2 180Β°Cable outlet 1 pack = 1 unit",60.300000000000004,"ST",1,"SIMATIC",0.03,1,"6AG19011BB107AA0"]
["6AG1901-1BB20-7AA0","SIPLUS NET RJ45 plug 90 2x2 -40...+70Β°C with conformal coating based on 6GK1901-1BB20-2AA0 . RJ45 plug-in connector (10/100 Mbit/s) with rugged Metal enclosure and FC connection system for IE FC Cable 2x2, 90Β° cable outlet 1 pack = 1 unit",60.300000000000004,"ST",1,"SIMATIC",0.03,1,"6AG19011BB207AA0"]
["6AG1931-2BA00-3AA0","SIPLUS PS 24 V/0.375 A Condensation permissible in: 48...220 V DC out: 24 V DC/0.375 A based on 6EP1731-2BA00",227,"ST",1,"SIMATIC",0.11,1,"6AG19312BA003AA0"]
["6AG1931-2EC21-2AA0","SIPLUS PS DC-UPS 24 V/15 A -25...+60Β°C based on 6EP1931-2EC21",397,"ST",1,"SIMATIC",0.4,1,"6AG19312EC212AA0"]
["6AG1931-2FC21-7AA0","SIPLUS PS DC UPS module 24 V/40 A -25...+70Β°C with conformal coating based on 6EP1931-2FC21 . Uninterruptible Power supply without interface Input: 24 V DC/43 A Output: 24 V DC/40 A",714,"ST",1,"SIMATIC",1.1000000000000001,1,"6AG19312FC217AA0"]
["6AG1950-2AA01-4AA0","SIPLUS SIWAREX U electronic weighing system for medial exposure based on 7MH4950-2AA01",2111,"ST",1,"SIMATIC",0.224,1,"6AG19502AA014AA0"]
["6AG1952-1AL00-4AA0","SIPLUS S7-400 RAM Card 2 MB for medial exposure based on 6ES7952-1AL00-0AA0",1281,"ST",1,"SIMATIC",5.1999999999999998E-2,1,"6AG19521AL004AA0"]
["6AG1952-1AM00-7AA0","SIPLUS S7-400 MC RAM 4 MB -25...+70Β°C with conformal coating based on 6ES7952-1AM00-0AA0 . RAM Memory Card for S7-400, long type of construction, 4 MB",1995,"ST",1,"SIMATIC",5.5E-2,1,"6AG19521AM007AA0"]
["6AG1952-1AP00-7AA0","SIPLUS S7-400 MC RAM 8 MB -25...+70Β°C with conformal coating based on 6ES7952-1AP00-0AA0 . RAM Memory Card for S7-400, long type of construction, 8 Byte",3371,"ST",1,"SIMATIC",5.5E-2,1,"6AG19521AP007AA0"]
["6AG1952-1AS00-7AA0","SIPLUS S7-400 MC RAM 16 MB -25...+70Β°C with conformal coating based on 6ES7952-1AS00-0AA0 . RAM Memory Card for S7-400, long type of construction, 16 Byte",5009,"ST",1,"SIMATIC",5.5E-2,1,"6AG19521AS007AA0"]
["6AG1952-1AY00-7AA0","SIPLUS S7-400 MC RAM 64 MB -25...+70Β°C with conformal coating based on 6ES7952-1AY00-0AA0 . RAM Memory Card for S7-400, long type of construction, 64 Byte",5387,"ST",1,"SIMATIC",5.5E-2,1,"6AG19521AY007AA0"]
["6AG1952-1KT00-4AA0","SIPLUS S7-400 flash EPROM card for medial exposure with conformal coating based on 6ES7952-1KT00-0AA0",3329,"ST",1,"SIMATIC",4.7E-2,1,"6AG19521KT004AA0"]
["6AG1960-1AA04-7AA0","SIPLUS S7-400 optical fiber cable 1 m HF-S -25...+70Β°C . Patch cable FOC 1 m for synchronization module",110,"ST",1,"SIMATIC",2.9000000000000001E-2,1,"6AG19601AA047AA0"]
["6AG1960-1AA04-7BA0","SIPLUS S7-400 optical fiber cable 2 m HF-S -25...+70Β°C . Patch cable FOC 2 m for synchronization module",154,"ST",1,"SIMATIC",4.2000000000000003E-2,1,"6AG19601AA047BA0"]
["6AG1960-1AA04-7KA0","SIPLUS S7-400 optical fiber cable 10 m HF- -25...+70Β°C . Patch cable FOC 10 m for synchronization module",173,"ST",1,"SIMATIC",0.157,1,"6AG19601AA047KA0"]
["6AG1960-1AA06-7XA0","SIPLUS S7-400 Sync module near -25...+70Β°C with conformal coating based on 6ES7960-1AA06-0XA0 . Synchronization module V6 for patch cable to 10 m",690,"ST",1,"SIMATIC",0.1,1,"6AG19601AA067XA0"]
["6AG1960-1AB06-7XA0","SIPLUS S7-400 Sync module remote -25...+70Β°C with conformal coating based on 6ES7960-1AB06-0XA0 . Synchronization module V6 for cable up to 10 km",1061,"ST",1,"SIMATIC",0.1,1,"6AG19601AB067XA0"]
["6AG1961-2BA31-7AA0","SIPLUS PS PSE200U 3A with conformal coating based on 6EP1961-2BA31 . Selectivity module 4-channel input: 24 V DC output: 24 V DC/3 A per channel Output current adjustable 0.5-3 with status message per channel",300,"ST",1,"SIMATIC",0.17,1,"6AG19612BA317AA0"]
["6AG1961-2BA41-7AA0","SIPLUS PS PSE200U 10 A with conformal coating based on 6EP1961-2BA41 . SELECTIVITY module 4-channel 4-channel input: 24 V DC Output: 24 V DC/10 A per channel output current adjustable 3-10 with status message per channel",318,"ST",1,"SIMATIC",0.22,1,"6AG19612BA417AA0"]
["6AG1961-3BA01-7AA0","SIPLUS PS modular buffer module -25...+70Β°C with conformal coating based on 6EP1961-3BA01 . for 6EP1x 3x-3BAX0 Buffer time 100 ms to 10 s depending on load current",382,"ST",1,"SIMATIC",1.2,1,"6AG19613BA017AA0"]
["6AG1961-3BA21-4AX0","SIPLUS PS E202U redundancy module for medial exposure with conformal coating based on 6EP1961-3BA21 . Input/output: 24 V DC/40 A suitable for decoupling two SITOP power supplies with max. 20 A output current each",280,"ST",1,"SIMATIC",0.41099999999999998,1,"6AG19613BA214AX0"]
["6AG1961-3BA21-7AX0","SIPLUS PS E202U redundancy module -40...+70Β°C with conformal coating based on 6EP1961-3BA21 . Input/output: 24 V DC/40 A suitable for decoupling two SITOP power supplies with max. 20 A output current each",363,"ST",1,"SIMATIC",0.41099999999999998,1,"6AG19613BA217AX0"]
["6AG1964-2AA04-7AB0","SIPLUS S7-400 IF 964-DP -25...+70Β°C with conformal coating based on 6ES7964-2AA04-0AB0 . Interface module DP master",1134,"ST",1,"SIMATIC",0.112,1,"6AG19642AA047AB0"]
["6AG1971-0AA00-7AA0","SIPLUS S7-400 battery box PS 40 -25...+70Β°C with conformal coating based on A5E00753961 Battery box for additional RAM buffering of the S7-400 with use of a standard lithium cell of type of construction D (mono cell), battery not included in scope of delivery",448,"ST",1,"SIMATIC",0.26800000000000002,1,"6AG19710AA007AA0"]
["6AG1972-0AA02-7XA0","SIPLUS DP RS-485-Repeater -25...+70Β°C with conformal coating based on 6ES7972-0AA02-0XA0 . For connection of PROFIBUS/MPI bus systems with max. 31 nodes max. baud rate 12 Mbit/s, Β° of protection IP20",579,"ST",1,"SIMATIC",0.28899999999999998,1,"6AG19720AA027XA0"]
["6AG1972-0AB01-4XA0","SIPLUS DP diagnostics repeater for medial exposure with conformal coating based on 6ES7972-0AB01-0XA0",1355,"ST",1,"SIMATIC",0.32500000000000001,1,"6AG19720AB014XA0"]
["6AG1972-0BA12-2XA0","SIPLUS DP PROFIBUS connector M R-90Β°Cable outlet -25...+70Β°C with conformal coating based on 6ES7972-0BA12-0XA0",85,"ST",1,"SIMATIC",0.05,1,"6AG19720BA122XA0"]
["6AG1972-0BA42-7XA0","SIPLUS DP PB CONNECTOR W R - TILTED CABLE OUTLET -40 ... +70 Β°C with conformal coating based on 6ES7972-0BA41-0XA0",94.3,"ST",1,"SIMATIC",5.0999999999999997E-2,1,"6AG19720BA427XA0"]
["6AG1972-0BB12-2XA0","SIPLUS DP PROFIBUS connector M R + PG 90Β°Cable outlet -25...+70Β°C with conformal coating based on 6ES7972-0BB12-0XA0",87.199999999999989,"ST",1,"SIMATIC",0.06,1,"6AG19720BB122XA0"]
["6AG1972-0BB42-7XA0","SIPLUS DP PB-CONNECTOR WITH R - W PG - ANGLED -40 ... +70Β°C with conformal coating based on 6ES7972-0BB42-0XA0",109,"ST",1,"SIMATIC",5.0999999999999997E-2,1,"6AG19720BB427XA0"]
["6AG1972-0BB70-7XA0","SIPLUS DP PB connector PG socket 90Β°Cable outlet -40...+70Β°C with conformal coating based on 6ES7972-0BB70-0XA0 . Connection plug for PROFIBUS up to 12 Mbit/s",122,"ST",1,"SIMATIC",5.0999999999999997E-2,1,"6AG19720BB707XA0"]
["6AG1972-0DA00-2AA0","SIPLUS DP Terminator RS485 -25...+60Β°C based on 6ES7972-0DA00-0AA0",181,"ST",1,"SIMATIC",0.106,1,"6AG19720DA002AA0"]
["6AG2124-0GC13-1AX0","SIPLUS HMI TP700 OUTDOOR RAIL -25Β°C...60Β°C T1 with 70Β°C for 10 min with conformal coating based on 6AV2124-0GC13-0AX0. TP700 Comfort Outdoor, Comfort \"Panel, Touch operation, 7\"\"\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 12 MB configuration memory, Windows CE 6.0, configurable WINCC Comfort V13 SP1 and higher, HSP",3108,"ST",1,"SIMATIC",1.5609999999999999,1,"6AG21240GC131AX0"]
["6AG2124-0QC13-1AX0","SIPLUS HMI TP1500 OUTDOOR T1 RAIL -25 ... +60Β°C with conformal coating based on 6AV2124-0QC13-0AX0 . touch \"operation, 15\"\"\" Widescreen-TFT-Display, 16 MIL. colors, PROFINET INTERFACE, MPI/PROFIBUS DP INTERFACE, 12 MB USER MEMORY, WINDOWS CE 6.0, configurable from WINCC COMFORT V13 SP1, HSP",8316,"ST",1,"SIMATIC",6.2,1,"6AG21240QC131AX0"]
["6AG2131-6BH01-4BA0","SIPLUS ET 200SP DI 16X24VDC ST TX RAIL -40Β…+70Β°C TX with 85Β°C for 10min with conformal coating based on 6ES7131-6BH01-0BA0 . type 3 (IEC 61131), sink input, (PNP, P-reading), Packing unit: 1 Piece, fits to BU-type A0, Colour Code CC00, input delay time 0,05..20ms, diagnostics wire break, diagnostics supply voltage",174,"ST",1,"SIMATIC",3.6999999999999998E-2,1,"6AG21316BH014BA0"]
["6AG2131-6CF00-4AU0","SIPLUS ET 200SP DI 8x48VUC TX RAIL -40...+70 Β°C TX with 85 Β°C for 10 minutes with conformal coating based on 6ES7131-6CF00-0AU0 . digital input module, DI 8X 24V AC..48V UC Basic, Pack quantity: 1 unit, suitable for BU type U0, Color code CC20, Module diagnostics",205,"ST",1,"SIMATIC",5.8999999999999997E-2,1,"6AG21316CF004AU0"]
["6AG2131-6FD01-4BB1","SIPLUS ET 200SP DI 4X120/230VAC TX RAIL -40Β…+70Β°C TX with 85Β°C for 10min for Conformal Coating based on 6ES7131-6FD01-0BB1. Standard, type 3 (IEC 61131), Packing unit: 1 piece, fits to BU-type B1, Colour Code CC41, module diagnostics",137,"ST",1,"SIMATIC",4.5999999999999999E-2,1,"6AG21316FD014BB1"]
["6AG2131-6TF00-4CA0","SIPLUS ET 200SP DI 8x NAMUR HF TX RAIL -40 ... +70Β°C TX with 85Β°C for 10 minutes with conformal coating based on 6ES7131-6TF00-0CA0 . DI 8x NAMUR High Feature, suitable for BU type A0, Color code CC01, channel diagnostics",485,"ST",1,"SIMATIC",0.04,1,"6AG21316TF004CA0"]
["6AG2132-6BD20-4BA0","SIPLUS ET 200SP DQ 4X24VDC/2A ST TX RAIL -40 ... +70Β°C TX with 85Β°C for 10 minutes with conformal coating based on 6ES7132-6BD20-0BA0 . suitable for BU type A0, Color code CC02, Module diagnostics",142,"ST",1,"SIMATIC",3.6999999999999998E-2,1,"6AG21326BD204BA0"]
["6AG2132-6BF00-4CA0","SIPLUS ET 200SP DQ 8X24VDC/ 0.5A TX RAIL -40 ... +70Β°C TX with 85Β°C for 10 minutes with conformal coating based on 6ES7132-6BF00-0CA0 . Fits BU type A0, Color code CC02, Channel Diagnose",159,"ST",1,"SIMATIC",3.5999999999999997E-2,1,"6AG21326BF004CA0"]
["6AG2132-6BH01-4BA0","SIPLUS ET 200SP DQ 16X24VDC/ 0.5A TX RAIL -40Β…+70Β°C TX with 85Β°C for 10min with conformal coating based on 6ES7132-6BH01-0BA0 . (PNP,P-switching) Packing unit: 1 piece, fits to BU-type A0, Colour Code CC00, substitute value output, module diagnostics for: short-circuit to L+ and ground, wire break, supply voltage",203,"ST",1,"SIMATIC",3.6999999999999998E-2,1,"6AG21326BH014BA0"]
["6AG2132-6FD00-4CU0","SIPLUS ET 200SP DQ 4X24..230VAC TX RAIL -40...+70Β°C TX with 85Β°C for 10min with Conformal Coating based on 6ES7132-6FD00-0CU0 . digital output module packaging unit: 1 piece, two alternative modes: DQ and power control, fits to BU-Type U0, color code CC20, channel diagnosis",473,"ST",1,"SIMATIC",5.8999999999999997E-2,1,"6AG21326FD004CU0"]
["6AG2132-6GD51-4BA0","SIPLUS ET 200SP RQ 4x24VUC/2A ST TX RAIL -40Β…+70Β°C TX with 85Β°C for 10min with conformal coating based on 6ES7132-6GD51-0BA0 . 4 changeover contacts, isolated contacts, packing unit: 1 piece, fits to BU-type A0, Colour Code CC00, substitute value output, module diagnostics for: supply voltage",116,"ST",1,"SIMATIC",3.6999999999999998E-2,1,"6AG21326GD514BA0"]
["6AG2132-6HD01-4BB1","SIPLUS ET 200SP RQ 4x120VDC/230 TX RAIL -40Β…+70Β°C TX with 85Β°C for 10min with conformal coating based on 6ES7132-6HD01-0BB1 . 4 normally open contacts, isolated contacts, packing unit: 1 piece, fits to BU-type B0 and B1, Colour Code CC40, substitute value output, module diagnostics for: supply voltage",168,"ST",1,"SIMATIC",4.4999999999999998E-2,1,"6AG21326HD014BB1"]
["6AG2132-6MD00-4BB1","SIPLUS ET 200SP RQ 4x120/230V MA TX RAIL -40Β…+70Β°C TX with 85Β°C for 10min with conformal coating based on 6ES7132-6MD00-0BB1 . relay module normally open, with manual operation, packing unit VPE 1, suitable for BU type B0 or B1, Module diagnostics",273,"ST",1,"SIMATIC",3.5999999999999997E-2,1,"6AG21326MD004BB1"]
["6AG2134-6GD01-1BA1","SIPLUS ET 200SP AI 4XI 2-/4-wire T1 rail -25Β…+55Β°C T1 with 70Β°C for 10 minutes with conformal coating based on 6ES7134-6GD01-0BA1",342,"ST",1,"SIMATIC",0.04,1,"6AG21346GD011BA1"]
["6AG2134-6GD01-4BA1","SIPLUS ET 200SP AI 4xI 2-/4-w TX RAIL -40Β…+70Β°C TX with 85Β°C for 10min with conformal coating based on 6ES7134-6GD01-0BA1 . analog input module, AI 4XI 2-/4-Wire Standard, packing size: 1 piece, fits to BU-Typ A0, A1, module-diagnosis, 16 Bit, +/-0, color code CC03,",342,"ST",1,"SIMATIC",0.04,1,"6AG21346GD014BA1"]
["6AG2134-6GF00-4AA1","SIPLUS ET 200SP AI 8xI 2-/4-W BA TX RAIL -40...+70 Β°C TX with 85 Β°C for 10 minutes with conformal coating based on 6ES7134-6GF00-0AA1 . Analog input module, AI 8XI 2-/4-wire Basic, suitable for BU type A0, A1, Color code CC01, Module diagnostics, 16 bit",567,"ST",1,"SIMATIC",3.6999999999999998E-2,1,"6AG21346GF004AA1"]
["6AG2134-6HB00-1CA1","SIPLUS ET 200SP AI 2XU/I 2/4W HF T1 RAIL -25 ... +60Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7134-6HB00-0CA1 . AI 2X U/I 2-,4-WIRE HF, suitable for BU type A0, A1, Color code CC05, Channel diagnostics 16 bit, +/-0.1%",408,"ST",1,"SIMATIC",4.1000000000000002E-2,1,"6AG21346HB001CA1"]
["6AG2134-6HD01-1BA1","SIPLUS ET 200SP AI 4XU/I 2-WIRE T1 RAIL -25Β…+55Β°C T1 with 70Β°C for 10min with conformal coating based on 6ES7134-6HD01-0BA1",344,"ST",1,"SIMATIC",0.04,1,"6AG21346HD011BA1"]
["6AG2134-6HD01-4BA1","SIPLUS ET 200SP AI 4xU/I 2-w ST TX RAIL -40Β…+70Β°C TX with 85Β°C for 10min with conformal coating based on 6ES7134-6HD01-0BA1 . analog input module, AI 4XU/I 2-Wire Standard, packing unit: 1 piece, fits to BU-Typ A0, A1, color code CC03, module diagnosis, 16 Bit, +/-0,3%",344,"ST",1,"SIMATIC",0.04,1,"6AG21346HD014BA1"]
["6AG2134-6JF00-1CA1","SIPLUS ET 200SP AI 8XRTD/TC HF T1 RAIL -25Β°C...60Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7134-6JF00-0CA1. Analog input module, AI 8xRTD/TC 2-wire High Feature suitable for BU type A0, A1, Color code CC00, channel diagnostics, 16 bit, +/-0.1%",557,"ST",1,"SIMATIC",3.9E-2,1,"6AG21346JF001CA1"]
["6AG2134-6PA00-4CU0","SIPLUS ET 200SP AI EM 480V CT HF TX RAIL -40...+70 Β°C TX with 85 Β°C for 10 minutes with conformal coating based on 6ES7134-6PA00-0CU0 . for 1A or 5A current transformer, with network analysis functions, suitable for BU type U0, channel diagnostics",683,"ST",1,"SIMATIC",0.05,1,"6AG21346PA004CU0"]
["6AG2134-6PA20-4BD0","SIPLUS ET 200SP AI EMETER 480VA TX RAIL -40 ... +70Β°C(TX mit 85Β°C fΓΌr 10 Min) mit conformal coating based on 6ES7134-6PA20-0BD0 . ANALOG INPUT MODULE, AI ENERGY METER 480VAC ST, FITS TO BU-TYPE D0, CHANNEL DIAGNOSIS",408,"ST",1,"SIMATIC",5.3999999999999999E-2,1,"6AG21346PA204BD0"]
["6AG2135-6HD00-4BA1","SIPLUS ET 200SP AQ 4XU/I ST TX RAIL -40 ... +70Β°C TX with 85 Β°C for 10 minutes with conformal coating based on 6ES7135-6HD00-0BA1 . AQ 4XU/I Standard, suitable for BU type A0, A1, Color code CC00, Module diagnostics",434,"ST",1,"SIMATIC",0.04,1,"6AG21356HD004BA1"]
["6AG2136-6BA00-1CA0","SIPLUS ET 200SP F-DI 4/8X24 V DC RAIL -25 ... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7136-6BA00-0CA0 . 15 mm overall width, up to PL E (ISO 13849-1)/ SIL3 (IEC 61508)",520,"ST",1,"SIMATIC",0.09,1,"6AG21366BA001CA0"]
["6AG2136-6DB00-1CA0","SIPLUS ET 200SP F-DQ 4 x 24 V DC/2 A PM RAIL -25 ... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7136-6DB00-0CA0 . 15 mm overall width, up to PL E (ISO13849) up to SIL 3 (IEC 61508)",598,"ST",1,"SIMATIC",6.8000000000000005E-2,1,"6AG21366DB001CA0"]
["6AG2136-6PA00-1BC0","SIPLUS ET 200SP F-PM-E 24 V DC/8A PPM RAIL -25 ... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7136-6PA00-0BC0 . POWER M. F-PM-E PPM PROFIsafe, for ET \"200SP; 24 V DC safe shutdown of\" DQ and F-DQ up to PL D/SIL2 or PL E/SIL3 2 safe dig. inputs 1 safe dig. output PPM",680,"ST",1,"SIMATIC",8.1000000000000003E-2,1,"6AG21366PA001BC0"]
["6AG2136-6RA00-1BF0","SIPLUS ET 200SP F-RQ 24VDC230VAC/5A RAIL -25 ... +55Β°C T1 with 70Β°C for 10min with conformal coating based on 6ES7136-6RA00-0BF0",258,"ST",1,"SIMATIC",7.1999999999999995E-2,1,"6AG21366RA001BF0"]
["6AG2137-6AA00-1BA0","SIPLUS ET 200SP CM PTP T1 RAIL -25 ... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7137-6AA00-0BA0. CM PTP communication module for serial connection RS422, RS485 and RS232, Freeport, 3964 (R), USS, MODBUS RTU Master, Slave, 115200 Kbit/s",566,"ST",1,"SIMATIC",0.04,1,"6AG21376AA001BA0"]
["6AG2137-6BD00-1BA0","SIPLUS ET 200SP CM 4XIO-Link ST -25 ... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7137-6BD00-0BA0. CM 4xIO-Link ST Communication Module IO-Link master V1.1",438,"ST",1,"SIMATIC",3.7999999999999999E-2,1,"6AG21376BD001BA0"]
["6AG2138-6AA00-1BA0","SIPLUS ET 200SP TM COUNT 1X24 V T1 RAIL -25 ... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7138-6AA00-0BA0 . Counting Module, 1 channel for 24V Incremental encoder or 24V pulses, 3DI, 2DQ",364,"ST",1,"SIMATIC",5.2999999999999999E-2,1,"6AG21386AA001BA0"]
["6AG2138-6DB00-1BB1","SIPLUS ET 200SP TM PULSE 2x24V -25Β°C...60Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7138-6DB00-0BB1. PWM and pulse output 2 channels 2 A for proportional valves and DC motors",590,"ST",1,"SIMATIC",5.2999999999999999E-2,1,"6AG21386DB001BB1"]
["6AG2155-5AA00-1AC0","SIPLUS ET 200MP IM 155-5 PN HF T1 RAIL -25Β°C ... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7155-5AA00-0AC0 . PROFINET IO-DEVICE interface module IM 155-5 PN HF, for ET 200MP \"Elektronicmodules; up to 12\" IO-MODULES without additional \"PS; up to 30 IO- MODULES with\" \"additional PS SHARED DEVICE;2\" \"PORT-SWITCH; RJ45, SHARED\" \"DEVICE; MRP; IRT >=0,25MS;\" \"Isochronicity FW-update;\" \"I&M0...3; fast start up\" \"S2-Redundancy; SHARED DEVICE\" with 4 Controller",1145,"ST",1,"SIMATIC",0.35599999999999998,1,"6AG21555AA001AC0"]
["6AG2155-5AA01-4AB0","SIPLUS ET 200MP IM155-5 PN ST TX rail -40Β°C to +70Β°C with conformal coating based on 6ES7155-5AA01-0AB0 . PROFINET IO device Interface module IM 155-5 PN ST for ET 200MP \"electronic modules; up to 12 IO\" modules without PS up to 30 IO modules with additional PS \"integrated 2-port switch; RJ45\" \"shared device; MRP IRT >=0.25\" \"ms; Isochronous mode FW update;\" I&M0...3 FSU with 500 ms",1134,"ST",1,"SIMATIC",0.35899999999999999,1,"6AG21555AA014AB0"]
["6AG2155-6AA01-4BN0","SIPLUS ET 200SP IM155-6PN ST BA TX RAIL -40 ... +70Β°C (TX with 85Β°C for 10 min) with conformal coating based on 6ES7155-6AA01-0BN0 . max. 32 Peripherymodules and 16 ET 200AL Modules, Single Hot SWAP, Bundle contains: Interface-Module (6AG2155-6AU01-4BN0), Server-Module (6AG1193-6PA00-7AA0), Busadapter BA 2xRJ45",706,"ST",1,"SIMATIC",0.20100000000000001,1,"6AG21556AA014BN0"]
["6AG2155-6AU00-1CN0","SIPLUS ET 200SP IM155-6PN HF T1 RAIL -25 ... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7155-6AU00-0CN0 . ET 200SP IM155-6PN High-Feature Max. 64 Periphery Modules, 0.25 MS Isochronous Mode Multi Hot Swap, Incl. server module",570,"ST",1,"SIMATIC",0.2,1,"6AG21556AU001CN0"]
["6AG2155-6AU01-1CN0","SIPLUS ET 200SP IM155-6PN HF T1 rail -25...+55 Β°C T1 with 70 Β°C for 10 minutes With conformal coating Based on 6ES7155-6AU01-0CN0 . 2-port interface module IM 155-6PN/2 High Feature, 1 slot for BusAdapter, max. 64 I/O modules and 16 ET 200AL modules, S2 redundancy, multi hot swap, 0.25 ms, isochronous mode, optional PN strain relief, including server module",573,"ST",1,"SIMATIC",0.2,1,"6AG21556AU011CN0"]
["6AG2155-6AU01-4BN0","SIPLUS ET 200SP IM155-6PN ST TX RAIL -40 ... +70Β°C (TX with 85Β°C for 10 Min) WITH conformal coating based on 6ES7155-6AU01-0BN0 . max. 32 Peripherymodules, and 16 ET 200AL Modules, Single Hot SWAP, incl. Server-Module (6AG1193-6PA00-7AA0)",514,"ST",1,"SIMATIC",0.20100000000000001,1,"6AG21556AU014BN0"]
["6AG2158-3AD10-4XA0","SIPLUS PN/PN Coupler TX RAIL -40...+70Β°C TX with 85Β°C for 10min with conformal coating based on 6ES7158-3AD10-0XA0 . for deterministic data exchange between max.4 PN-Controller per subnet, also from subnet to subnet, PROFIsafe data exchange, I/O-, MSI-, MSO- and data record communication, redundant power supply, PN-connection via SIMATIC BusAdapter (BA), delivery w/o BusAdapter",1092,"ST",1,"SIMATIC",0.3,1,"6AG21583AD104XA0"]
["6AG2193-6AF00-4AA0","SIPLUS ET 200SP BA 2XFC TX RAIL -40 ... +70Β°C TX with 85Β°C for 10 minutes with conformal coating based on 6ES7193-6AF00-0AA0 . Bus Adapter BA 2xFC, 2x FastConnect terminals for PROFINET",193,"ST",1,"SIMATIC",6.3E-2,1,"6AG21936AF004AA0"]
["6AG2193-6AR00-4AA0","SIPLUS ET 200SP BA 2xRJ45 TX RAIL -40 ... +70Β°C TX with 85 Β°C for 10 minutes with conformal coating based on 6ES7193-6AR00-0AA0 . Bus Adapter BA 2x RJ45, 2 RJ45 connectors for PROFINET",242,"ST",1,"SIMATIC",5.5E-2,1,"6AG21936AR004AA0"]
["6AG2193-6BP00-4BA0","SIPLUS ET 200SP BU15-P16+A0+2B TX RAIL -40 ... +70Β°C TX with 85Β°C for 10 minutes with conformal coating based on 6ES7193-6BP00-0BA0 . BU type A0, Push-in terminals, without AUX terminals, bridged to the left, WxH: 15x117 mm",36.6,"ST",1,"SIMATIC",4.8000000000000001E-2,1,"6AG21936BP004BA0"]
["6AG2193-6BP00-4BD0","SIPLUS ET 200SP BU20-P12+A0+0B TX RAIL -40 ... +70Β°C TX with 85Β°C for 10 minutes with conformal coating based on 6ES7193-6BP00-0BD0 . BU type D0, Push-in terminals, w/o AUX terminals, bridged for links BU WxH: 20x117 mm",50.300000000000004,"ST",1,"SIMATIC",5.5E-2,1,"6AG21936BP004BD0"]
["6AG2193-6BP00-4BU0","SIPLUS ET 200SP BU20-P16+A0+2B TX RAIL -40...+70 Β°C TX with 85 Β°C for 10 minutes with conformal coating based on 6ES7193-6BP00-0BU0 . BU type U0, Pack quantity: 1 unit, Push-in terminals, without AUX terminals, bridged to the left, WxH: 20 mm x 117 mm",63,"ST",1,"SIMATIC",4.8000000000000001E-2,1,"6AG21936BP004BU0"]
["6AG2193-6BP00-4DA0","SIPLUS ET 200SP BU15-P16+A0+2D TX RAIL -40 ... +70Β°C TX with 85Β°C for 10 minutes with conformal coating based on 6ES7193-6BP00-0DA0 . BU type A0, Push-in terminals, without AUX terminals, New load group, WxH: 15x117 mm",64.699999999999989,"ST",1,"SIMATIC",1E-3,1,"6AG21936BP004DA0"]
["6AG2193-6BP00-4DA1","SIPLUS ET 200SP BU15-P16+A0+2D/T TX RAIL -40 ... +70Β°C TX with 85Β°C for 10 minutes with conformal coating based on 6ES7193-6BP00-0DA1. BU type A1, Push-in terminals, without AUX terminals, New load group, WxH: 15x117 mm with temperature acquisition",80.399999999999991,"ST",1,"SIMATIC",4.8000000000000001E-2,1,"6AG21936BP004DA1"]
["6AG2193-6BP00-4DU0","SIPLUS ET 200SP BU20-P16+A0+2D TX RAIL -40...+70 Β°C TX with 85 Β°C for 10 minutes with conformal coating based on 6ES7193-6BP00-0DU0 . BU type U0, Pack quantity: 1 unit, Push-in terminals, without AUX terminals, new potential group, WxH: 20 mm x 117 mm",94.5,"ST",1,"SIMATIC",4.8000000000000001E-2,1,"6AG21936BP004DU0"]
["6AG2193-6BP20-4BA0","SIPLUS ET 200SP BU15-P16+A10+2B TX RAIL -40 ... +70Β°C TX with 85Β°C for 10 minutes with conformal coating based on 6ES7193-6BP20-0BA0 . BU type A0, Push-in terminals, with 10 AUX terminals, bridged to the left, WxH: 15x141 mm",49.800000000000004,"ST",1,"SIMATIC",5.8999999999999997E-2,1,"6AG21936BP204BA0"]
["6AG2193-6BP20-4BB1","SIPLUS ET 200SP BU20-P12+A0+4B TX RAIL -40 ... +70Β°C TX with 85Β°C for 10 minutes with conformal coating based on 6ES7193-6BP20-0BB1 . BU type B1, push-in terminals, without auxiliary terminals, new load group, WxH: 15x117 mm, with temperature recording",64.899999999999991,"ST",1,"SIMATIC",5.7000000000000002E-2,1,"6AG21936BP204BB1"]
["6AG2193-6BP20-4BF0","SIPLUS ET 200SP BU20-P8+A4+0B TX RAIL -40 ... +85Β°C Tx mit 85Β°C fΓΌr 10 min with conformal coating based on 6ES7193-6BP20-0BF0 . BU-TYPE F0, PUSH-IN KLEMMEN, WITH AUX-TERMINALS, BRIDGED TO LEFT BU WXH: 20MMX117MM",57.800000000000004,"ST",1,"SIMATIC",5.7000000000000002E-2,1,"6AG21936BP204BF0"]
["6AG2193-6BP20-4DA0","SIPLUS ET 200SP BU15-P16+A10+2D TX RAIL -40 ... +70Β°C TX with 85Β°C for 10 minutes with conformal coating based on 6ES7193-6BP20-0DA0 . BU type A0, Push-in terminals, with 10 AUX terminals, New load group, WxH: 15x141 mm",61.7,"ST",1,"SIMATIC",5.8999999999999997E-2,1,"6AG21936BP204DA0"]
["6AG2193-6BP20-4DC0","SIPLUS ET 200SP BU20-P6+A2+4D TX RAIL -40 ... +70Β°C TX with 85Β°C for 10 minutes with conformal coating based on 6ES7193-6BP20-0DC0 . BU-Type C0, Push-In terminals, with 2 AUX terminals, New load group WxH: 20x117 mm",78,"ST",1,"SIMATIC",5.6000000000000001E-2,1,"6AG21936BP204DC0"]
["6AG2212-1AE40-1XB0","SIPLUS S7-1200 CPU 1212C DC/DC/DC T1 RAIL -25 ... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7212-1AE40-0XB0 . compact CPU, DC/DC/DC, Onboard I/O: 8 DI 24 V DC 6 DO 24 V DC 2 AI 0-10 V DC, Power supply: 20.4-28.8V DC Program/data memory 50 KB",632,"ST",1,"SIMATIC",0.34,1,"6AG22121AE401XB0"]
["6AG2214-1AG40-1XB0","SIPLUS S7-1200 CPU 1214C DC/DC/DC T1 RAIL -25 ... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7214-1AG40-0XB0 . compact CPU, DC/DC/DC, Onboard I/O: 14 \"DI 24 V DC; 10 DO 24 V DC; 2 AI\" 0-10 V DC, Power supply: 20.4-28.8V DC, Program/data memory 75 KB",765,"ST",1,"SIMATIC",0.42099999999999999,1,"6AG22141AG401XB0"]
["6AG2221-1BF32-1XB0","SIPLUS S7-1200 SM 1221 8DI T1 RAIL -25 ... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7221-1BF32-0XB0 . Digital input 8 DI, 24 V DC, Sink/Source",270,"ST",1,"SIMATIC",0.17,1,"6AG22211BF321XB0"]
["6AG2222-1BF32-1XB0","SIPLUS S7-1200 SM 1222 8DQ T1 RAIL -25 ... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7222-1BF32-0XB0 . Digital output 8 DQ, 24 V DC, transistor 0.5 A",270,"ST",1,"SIMATIC",0.18,1,"6AG22221BF321XB0"]
["6AG2222-1HF32-1XB0","SIPLUS S7-1200 SM1222 8DQ RLY T1 RAIL -25 ...+55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7222-1HF32-0XB0 . Digital output 8 DQ, relay 2 A",287,"ST",1,"SIMATIC",0.19,1,"6AG22221HF321XB0"]
["6AG2223-0BD30-1XB0","SIPLUS S7-1200 SB1223 2DI/2DQ T1 RAIL -25 ... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7223-0BD30-0XB0 . Digital input/output 2 DI 24 V DC/2 DQ 24 V DC",236,"ST",1,"SIMATIC",2.9000000000000001E-2,1,"6AG22230BD301XB0"]
["6AG2223-1BH32-1XB0","SIPLUS S7-1200 SM 1223 8DI/8DQ T1 RAIL -25 ... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7223-1BH32-0XB0 . Digital input/output SM 1223, 8 DI/8 DO, 8 DI 24 V DC, Sink/Source, 8 DO, transistor 0.5 A",383,"ST",1,"SIMATIC",0.21,1,"6AG22231BH321XB0"]
["6AG2223-1PL32-1XB0","SIPLUS S7-1200 SM 1223 16DI/16DQ RLY T1 RAIL -25 ... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7223-1PL32-0XB0. Digital input/output 16DI/16DQ, 16 DI 24 V DC, Sink/Source, 16DQ, relay 2 A",664,"ST",1,"SIMATIC",0.23,1,"6AG22231PL321XB0"]
["6AG2231-5PD32-1XB0","SIPLUS S7-1200 SM 1231 RTD T1 RAIL -25 ... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7231-5PD32-0XB0 . SIMATIC S7-1200, Analog input, SM 1231 RTD, 4xAI RTD module",676,"ST",1,"SIMATIC",0.20699999999999999,1,"6AG22315PD321XB0"]
["6AG2232-4HD32-1XB0","SIPLUS S7-1200 SM 1232 T1 RAIL -25 ... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7232-4HD32-0XB0. S7-1200, Analog output, SM 1232, 4 AO, +/-10 V, 14-bit resolution: or 0-20 mA, 13-bit resolution:",530,"ST",1,"SIMATIC",0.214,1,"6AG22324HD321XB0"]
["6AG2234-4HE32-1XB1","SIPLUS S7-1200 SM 1234 4AI/2AQ -25 ... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7234-4HE32-0XB0. SM 1234, 4 AI/2 AO, +/-10 V, 14-bit resolution or 0 (4)-20mA, 13-bit resolution",601,"ST",1,"SIMATIC",0.218,1,"6AG22344HE321XB1"]
["6AG2241-1AH32-1XB0","SIPLUS S7-1200 CM1241 RS232 T1 RAIL -25... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7241-1AH32-0XB0 . Communication module RS232, 9-pole D-sub (socket), supports Freeport",327,"ST",1,"SIMATIC",0.156,1,"6AG22411AH321XB0"]
["6AG2241-1CH30-1XB0","SIPLUS S7-1200 CB 1241 RS485 RAIL -25Β°C...60Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7241-1CH30-1XB0 . RS485, terminal block, supports Freeport",180,"ST",1,"SIMATIC",2.9000000000000001E-2,1,"6AG22411CH301XB0"]
["6AG2241-1CH32-1XB0","SIPLUS S7-1200 CM1241 RS422/485 T1 RAIL -25 ... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7241-1CH32-0XB0 . Communication module CM 1241, RS422/485, 9-pole D-sub (pin) supports Freeport",327,"ST",1,"SIMATIC",0.159,1,"6AG22411CH321XB0"]
["6AG2242-5DX30-1XE0","SIPLUS S7-1200 CM 1242-5 T1 RAIL -25 ... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6GK7242-5DX30-0XE0 . Communication module CM 1242-5, for connecting S7-1200 to PROFIBUS as DP Slave module",676,"ST",1,"SIMATIC",0.17199999999999999,1,"6AG22425DX301XE0"]
["6AG2243-1BX30-1XE0","SIPLUS S7-1200 CP 1243-1 RAIL -25 ... +70Β°C (T1 with 70Β°C for 10 Min) with conformal coating based on 6GK7243-1BX30-0XE0",1061,"ST",1,"SIMATIC",0.17899999999999999,1,"6AG22431BX301XE0"]
["6AG2243-5DX30-1XE0","SIPLUS S7-1200 CM 1243-5 T1 RAIL -25 ... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6GK7243-5DX30-0XE0 . Communication module CM 1243-5 for connecting S7-1200 to PROFIBUS as DP master module",844,"ST",1,"SIMATIC",0.193,1,"6AG22435DX301XE0"]
["6AG2333-0SB00-4AY0","SIPLUS PS PSU2600 24V/5A TX rail -40...+70 Β°C with conformal coating . Stabilized power supply Input: 110 V DC Output: 24 V DC/5 A",389,"ST",1,"SIMATIC",0.5,1,"6AG23330SB004AY0"]
["6AG2510-1DJ01-1AB0","SIPLUS ET 200SP CPU 1510SP-1 PN -25 ... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7510-1DJ01-0AB0. Central processing unit with Work memory 100 KB for program and 750 KB for data, 1st interface: PROFINET IRT with 3-port switch, 72 ns bit performance, SIMATIC Memory Card required, Bus Adapter required for Port 1 and 2",1302,"ST",1,"SIMATIC",0.5,1,"6AG25101DJ011AB0"]
["6AG2510-1DJ01-4AB0","SIPLUS ET 200SP CPU 1510SP-1 PN RAIL -40...+70 Β°C TX with 85 Β°C for 10 minutes With conformal coating based on 6ES7510-1DJ01-0AB0 . Central processing unit with 100 KB work memory for program and 750 KB for data, 1st interface: PROFINET IRT 72 ns bit performance, SIMATIC memory card required, no pluggable BusAdapter",1565,"ST",1,"SIMATIC",0.91600000000000004,1,"6AG25101DJ014AB0"]
["6AG2510-1SJ01-1AB0","SIPLUS ET 200SP CPU 1510 F-1 PN T1 RAIL -25 ... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7510-1SJ01-0AB0 . CPU with RAM 150 KB for program and 750 KB for data 1st interface: PROFINET IRT with 3-port switch, 72 NS BIT Performance, SIMATIC Memory Card required, Bus adapter required for PORT 1 and 2",1890,"ST",1,"SIMATIC",0.5,1,"6AG25101SJ011AB0"]
["6AG2511-1AK01-4AB0","SIPLUS S7-1500 CPU 1511-1 PN TX RAIL -40 ... +70Β°C TX with 85Β°C for 10 min with conformal coating based on 6ES7511-1AK01-0AB0 . Central processing unit with RAM 150 KB for program and 1 MB for data, 1st interface: PROFINET IRT with 2-PORT SWITCH, 60 ns bit performance, SIMATIC Memory Card required without display",2153,"ST",1,"SIMATIC",0.50700000000000001,1,"6AG25111AK014AB0"]
["6AG2511-1AK02-1AB0","SIPLUS S7-1500 CPU 1511-1 PN T1 rail -25Β…+55Β°C T1 at 70Β°C for 10 min with conformal coating based on 6ES7511-1AK02-0AB0 . Central processing unit with Work memory 150 KB for program and 1 MB for data, 1st interface: PROFINET IRT with 2-port switch, 60 ns bit performance, SIMATIC Memory Card required",1355,"ST",1,"SIMATIC",0.50700000000000001,1,"6AG25111AK021AB0"]
["6AG2512-1DK01-1AB0","SIPLUS ET 200SP CPU 1512SP-1 PN -25 ... +60Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7512-1DK01-0AB0. Central processing unit with Work memory 200 KB for program and 1 MB for data, 1st interface: PROFINET IRT with 3-port switch, 48 ns bit performance, SIMATIC Memory Card required, Bus Adapter required for Port 1 and 2",1638,"ST",1,"SIMATIC",0.5,1,"6AG25121DK011AB0"]
["6AG2512-1DK01-4AB0","SIPLUS ET 200SP CPU 1512SP-1 PN RAIL -40...+70 Β°C TX with 85 Β°C for 10 minutes With conformal coating based on 6ES7512-1DK01-0AB0 . Central processing unit with 200 KB work memory for program and 1 MB for data, 1st interface: PROFINET IRT 48 ns bit performance, SIMATIC memory card required, no pluggable BusAdapter",1985,"ST",1,"SIMATIC",0.47,1,"6AG25121DK014AB0"]
["6AG2512-1SK01-1AB0","SIPLUS ET 200SP CPU 1512 F-1 PN T1 RAIL -25 ... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7512-1SK01-0AB0 . CPU with RAM 300 KB for program and 1 MB for data 1st interface: PROFINET IRT with 3-port switch, 48 NS BIT Performance, SIMATIC Memory Card required, Bus Adapter required for Port 1 and 2",2468,"ST",1,"SIMATIC",0.41499999999999998,1,"6AG25121SK011AB0"]
["6AG2515-2RM00-4AB0","SIPLUS S7-1500 CPU 1515R-2 PN TX RAIL -40...+70Β°C TX with 85Β°C for 10min with Conformal Coating based on 6ES7515-2RM00-0AB0 . central processing unit with working memory 500 KB for program and 3 MB data, 1. interface: PROFINET RT with 2 port switch, 2. interface PROFINET RT, SIMATIC memory card necessary",6290,"ST",1,"SIMATIC",0.91500000000000004,1,"6AG25152RM004AB0"]
["6AG2516-3AN01-4AB0","SIPLUS S7-1500 CPU 1516-3 PN/DP TX RAIL -40 ... +70Β°C TX with 85Β°C for 10 min with conformal coating based on 6ES7516-3AN01-0AB0 . CPU without display with 1 MB RAM for program and 5MB for data, 1st interface: PROFINET IRT with 2-port switch, 2nd interface: Ethernet, 3rd interface: PROFIBUS, 10 ns bit performance, SIMATIC Memory Card required",7634,"ST",1,"SIMATIC",0.9,1,"6AG25163AN014AB0"]
["6AG2516-3FN01-1AB0","SIPLUS S7-1500 CPU 1516F-3 PN/DP T1 RAIL -25 ... +55Β°C T1 70Β°C fΓΌr 10 min with conformal coating based on 6ES7516-3FN01-0AB0 . central processing unit with working memmory 1,5 MB for programm 5 MB for data, 1. INTERFACE: PROFINET IRT WITH 2 PORT SWITCH, 2. INTERFACE: ETHERNET 3. INTERFACE: PROFIBUS, 10 NS BIT-PERFORMANCE, SIMATIC MEMORY CARD NECESSARY",8474,"ST",1,"SIMATIC",0.93600000000000005,1,"6AG25163FN011AB0"]
["6AG2521-1BH00-4AB0","SIPLUS S7-1500 DI 16x24 V DC HF TX RAIL -40 ... +70Β°C TX with 85Β°C for 10 minutes with conformal coating based on 6ES7521-1BH00-0AB0 . 16 channels in groups of 16 Input \"delay 0,05 ... 20ms; Input type\" \"3 (IEC 61131); diagnostics,\" Hardware interrupts",376,"ST",1,"SIMATIC",0.28999999999999998,1,"6AG25211BH004AB0"]
["6AG2521-7EH00-4AB0","SIPLUS S7-1500 DI 16x110VDC HF TX RAIL -40 ... +70Β°C TX with 85Β°C for 10 min with conformal coating based on 6ES7521-7EH00-0AB0 . DI 16x24 ... 125V UC HF, 16 channels in groups of 1 Input delay 0,05 ... 20ms Input type 3 (IEC \"61131); diagnostics, Hardware\" interrupts",911,"ST",1,"SIMATIC",0.27100000000000002,1,"6AG25217EH004AB0"]
["6AG2522-1BH01-4AB0","SIPLUS S7-1500 DQ 16x24 V DC HF TX RAIL -40 ... +70Β°C TX with 85Β°C for 10 min with conformal coating based on 6ES7522-1BH01-0AB0 . 16 channels in groups of 8 4 A per \"group; Single-channel\" \"diagnostics; Substitute value\"",375,"ST",1,"SIMATIC",0.29099999999999998,1,"6AG25221BH014AB0"]
["6AG2522-5EH00-4AB0","SIPLUS S7-1500 DQ 16x110VDC ST TX RAIL -40 ... +70Β°C TX with 85Β°C for 10 min with conformal coating based on 6ES7522-5EH00-0AB0 . DQ 16x24 \"... 48VUC/125VDC/ 0.5A; 16\" channels in groups of 1, 0.5 A \"per group; substitute value;\" Observe derating",1344,"ST",1,"SIMATIC",0.2,1,"6AG25225EH004AB0"]
["6AG2522-5HF00-1AB0","SIPLUS S7-1500 DQ 8x230V AC ST 5A T1 RAIL -25 ... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7522-5HF00-0AB0 . DQ 8xAC \"230V/5A; relay; 8 channels in\" \"groups of 1 5 A per group;\" \"diagnostics; Substitute value\"",633,"ST",1,"SIMATIC",0.40500000000000003,1,"6AG25225HF001AB0"]
["6AG2526-1BH00-1AB0","SIPLUS S7-1500 F DI 16X24VDC HF T1 RAIL -25 ... +55Β°C T1 (70Β°C for 10 min) with conformal coating based on 6ES7526-1BH00-0AB0 . FAILSAFE DIGITAL INPUT MODULE, F-DI \"16X24VDC PROFISAFE; 35 MM\" \"WIDTH; UP TO PL E (ISO\" 13849-1)/ SIL3 (IEC 61508)",1250,"ST",1,"SIMATIC",0.09,1,"6AG25261BH001AB0"]
["6AG2526-2BF00-1AB0","SIPLUS S7-1500 F DQ 8x24VDC 2A T1 RAIL -25 ... +55Β°C T1 70Β°C for 10 min with conformal coating based on 6ES7526-2BF00-0AB0 . FAILSAFE digital output module F-DQ \"8X24VDC 2A PPM PROFISAFE; 35MM\" \"WIDTH; up to PL E (ISO\" 13849-1)/ SIL3 (IEC 61508)",1407,"ST",1,"SIMATIC",0.09,1,"6AG25262BF001AB0"]
["6AG2531-7KF00-4AB0","SIPLUS S7-1500 AI 8xU/I/RTD/TC TX RAIL -40 ... +70Β°C T1 with 85Β°C for 10 min with conformal coating based on 6ES7531-7KF00-0AB0 . analog input module AI 8 X U/I/RTD/TC ST, 16 bits of resolution, \"accuracy 0.3 %; 8 chnnels in\" \"groups of 8; 4 channels for RTD\" measuring, COMMON MODE VOLTAGE \"APPR. 10 V; DIAGNOSIS,\" PROCESSALARMS INCL. INFEED ELEMENT, SHIELD CLAMP AND SHIELD TERMINAL",1155,"ST",1,"SIMATIC",0.437,1,"6AG25317KF004AB0"]
["6AG2531-7NF10-4AB0","SIPLUS S7-1500 AI 8xU/I HS TX RAIL -40 ... +70Β°C TX with 85Β°C for 10 min with conformal coating based on 6ES7531-7NF10-0AB0 . 16 Bits of Resolution, Accuracy 0.3 \"Percent; 8 Channels in Groups\" \"of 8; Common Mode Voltage\" \"Appr.10V; Diagnosis,\" \"Processalarms; 8 Channels in\" 0.0625 ms incl. Infeed element, Shield Clamp and Shield Terminal",1313,"ST",1,"SIMATIC",0.42899999999999999,1,"6AG25317NF104AB0"]
["6AG2532-5HD00-4AB0","SIPLUS S7-1500 AQ 4xU/I ST TX RAIL -40 ... +70Β°C Tx with 85Β°C for 10 min with conformal coating based on 6ES7532-5HD00-0AB0 . 16 Bits of \"Resolution, Accuracy 0.3 %; 4\" \"Channels in Groups of 4; incl.\" Infeed element, Shield Clamp and Shield Terminal Diagnosis, Substitute value",1124,"ST",1,"SIMATIC",0.41499999999999998,1,"6AG25325HD004AB0"]
["6AG2541-1AB00-4AB0","SIPLUS S7-1500 CM PTP RS 422/485 TX rail -40...+70Β°C TX with 85Β°C for 10 minutes with conformal coating based on 6ES7541-1AB00-0AB0 . Communication module for serial connection RS 422 and RS 485, Freeport, 3964 (R), USS, MODBUS RTU master, slave, 115200 Kbit/s, 15-pin D-sub socket",1565,"ST",1,"SIMATIC",0.27300000000000002,1,"6AG25411AB004AB0"]
["6AG2541-1AD00-4AB0","SIPLUS S7-1500 CM PtP RS232 HF TX RAIL with conformal coating based on 6ES7541-1AD00-0AB0 -40...70Β°C (Tx with 85Β°C for 10 min) . HF Communictionmodul for SERIAL CONNECTION RS232, FREEPORT, 3964(R), USS, MODBUS RTU MASTER, SLAVE, 115200 KBIT/S, 9-PIN SUB-D CONNECTOR",1544,"ST",1,"SIMATIC",0.26900000000000002,1,"6AG25411AD004AB0"]
["6AG2542-6VX00-4XE0","SIPLUS ET 200SP CP 1542SP-1 IRC TX RAIL -40...+70Β°C TX with 85Β°C for 10min with conformal coating based on 6GK7542-6VX00-0XE0 . for connection of an SIMATIC S7-ET 200SP to Industrial Ethernet, SINAUT ST7, TeleControl Server Basic, IEC-60870-5-104 or DNP3 \"protocol to a control center;\" Open IE communication (TCP/IP, ISO-on-TCP, UDP), IP broadcast/multicast, SNMPV1, DHCP, Secure e-Mail, IPV4/IPV6, support of SINEMA Remote Connect",1943,"ST",1,"SIMATIC",0.20100000000000001,1,"6AG25426VX004XE0"]
["6AG2543-6WX00-4XE0","SIPLUS ET 200SP CP 1543SP-1 ISEC TX RAIL -40...+70Β°C TX mit 85Β°C for 10min with conformal coating based on 6GK7543-6WX00-0XE0 .",1838,"ST",1,"SIMATIC",0.20200000000000001,1,"6AG25436WX004XE0"]
["6AG2620-0AA00-4AA0","SIPLUS PN/CAN LINK TX RAIL -40 ... +70Β°C TX with 85Β°C for 10 min with conformal coating based on 6BK1620-0AA00-0AA0. Module for PROFINET to CAN or CANopen Fieldbus CAN 2.0A/B CANopen Manager or Slave according CiA301/302 IP20",913,"ST",1,"SIMATIC",0.22,1,"6AG26200AA004AA0"]
["6AG2623-0AA00-4AA0","SIPLUS PN/J1939 LINK TX RAIL -40...+70Β°C TX with 85Β°C for 10min with Conformal Coating based on 6BK1623-0AA00-0AA0 . gateway from Profinet to J1939 networks, IP20",935,"ST",1,"SIMATIC",1E-3,1,"6AG26230AA004AA0"]
["6AG2647-0AH11-1AX0","SIPLUS HMI KP300 Basic mono \"3,6\"\" T1 RAIL -25 ... +55Β°C T1\" at 70Β°C for 10 min with conformal coating based on 6AV6647-0AH11-3AX0 . Basic \"Panel, key operation, 3\"\" FSTN\" LCD display, Black/white, PROFINET interface, configurable from WinCE Basic V11/ STEP 7 Basic V11, contains open source software, which is provided free of charge See enclosed CD-ROM",769,"ST",1,"SIMATIC",0.375,1,"6AG26470AH111AX0"]
["6AG2677-2DB42-2GB0","SIPLUS ET 200SP CPU1515SP PC2 RAIL -40...+60Β°C T1 with 70Β°C for 10min with Conformal Coating based on 6ES7677-2DB42-0GB0 . 8 GB RAM, 30 GB CFast with Windows 10 IoT Enterprise 64 bit and S7-1500 Software Controller CPU 1505SP pre-installed, Interfaces: 1x slot CFast, 1x slot SD/MMC, 1x connection for ET 200SP bus adapter PROFINET, 1x 10/100/1000 Mbit/s Ethernet 2x USB 3.0; 2x USB 2.0, 1x display port,",4148,"ST",1,"SIMATIC",0.83,1,"6AG26772DB422GB0"]
["6AG4012-1AA10-0XX0","SIMATIC IPC347E (Rack PC, 19\", 4HU); Pentium Dual Core 3420 (2C/2T, 3.2 GHz, 3 MB cache); Interfaces: 2x Gbit Ethernet, 1x DVI-D, 1x VGA, 2x USB on the front, 4x USB on the rear, 1x USB internal, 2x serial, 2x PS/2, audio; 1x 500 GB HDD, internal; 2 GB DDR3 SD-RAM (1x 2 GB), single channel; without operating system; 100/240 V industrial power supply, without line cable",1381,"ST",1,"SIMATIC",17,1,"6AG40121AA100XX0"]
["6AG4012-1AA21-0BX0","SIMATIC IPC347E (Rack PC, 19\", 4HU); Pentium Dual Core 3420 (2C/2T, 3.2 GHz, 3 MB cache); Interfaces: 2x Gbit Ethernet, 1x DVI-D, 1x VGA, 2x USB on the front, 4x USB on the rear, 1x USB internal, 2x serial, 2x PS/2, audio; 1x 500 GB HDD, internal; 4 GB DDR3 SD-RAM (1x 4 GB), single channel; DVD +/-RW; Windows 7 Ultimate 64 bit SP1; 100/240 V industrial power supply, without line cable",2161,"ST",1,"SIMATIC",17,1,"6AG40121AA210BX0"]
["6AG4012-1AA21-0CX0","SIMATIC IPC347E (Rack PC, 19\", 4HU); Pentium Dual Core 3420 (2C/2T, 3.2 GHz, 3 MB cache); Interfaces: 2x Gbit Ethernet, 1x DVI-D, 1x VGA, 2x USB on the front, 4x USB on the rear, 1x USB internal, 2x serial, 2x PS/2, audio; 1x 500 GB HDD, internal; 4 GB DDR3 SD-RAM (1x 4 GB), single channel; DVD +/-RW; Windows10 Enterprise LTSB 2016; 100/240 V industrial power supply, without line cable",1933,"ST",1,"SIMATIC",17,1,"6AG40121AA210CX0"]
["6AG4012-1AA21-0XX0","SIMATIC IPC347E (Rack PC, 19\", 4HU); Pentium Dual Core 3420 (2C/2T, 3.2 GHz, 3 MB cache); Interfaces: 2x Gbit Ethernet, 1x DVI-D, 1x VGA, 2x USB on the front, 4x USB on the rear, 1x USB internal, 2x serial, 2x PS/2, audio; 1x 500 GB HDD, internal; 4 GB DDR3 SD-RAM (1x 4 GB), single channel; DVD +/-RW; without operating system; 100/240 V industrial power supply, without line cable",1640,"ST",1,"SIMATIC",17,1,"6AG40121AA210XX0"]
["6AG4012-1CA21-0BX0","SIMATIC IPC347E (Rack PC, 19\", 4HU); Core I5-4570S (4C/4T, 2.9 (3.6) GHz, 6 MB cache); Interfaces: 2x Gbit Ethernet, 1x DVI-D, 1x VGA, 2x USB on the front, 4x USB on the rear, 1x USB internal, 2x serial, 2x PS/2, audio; 1x 500 GB HDD, internal; 4 GB DDR3 SD-RAM (1x 4 GB), single channel; DVD +/-RW; Windows 7 Ultimate 64 bit SP1; 100/240 V industrial power supply, without line cable",2567,"ST",1,"SIMATIC",17,1,"6AG40121CA210BX0"]
["6AG4012-1CA21-0CX0","SIMATIC IPC347E (Rack PC, 19\", 4HU); Core I5-4570S (4C/4T, 2.9 (3.6) GHz, 6 MB cache); Interfaces: 2x Gbit Ethernet, 1x DVI-D, 1x VGA, 2x USB on the front, 4x USB on the rear, 1x USB internal, 2x serial, 2x PS/2, audio; 1x 500 GB HDD, internal; 4 GB DDR3 SD-RAM (1x 4 GB), single channel; DVD +/-RW; Windows10 Enterprise LTSB 2016; 100/240 V industrial power supply, without line cable",2339,"ST",1,"SIMATIC",17,1,"6AG40121CA210CX0"]
["6AG4012-1CA21-0XX0","SIMATIC IPC347E (Rack PC, 19\", 4HU); Core I5-4570S (4C/4T, 2.9 (3.6) GHz, 6 MB cache); Interfaces: 2x Gbit Ethernet, 1x DVI-D, 1x VGA, 2x USB on the front, 4x USB on the rear, 1x USB internal, 2x serial, 2x PS/2, audio; 1x 500 GB HDD, internal; 4 GB DDR3 SD-RAM (1x 4 GB), single channel; DVD +/-RW; without operating system; 100/240 V industrial power supply, without line cable",2046,"ST",1,"SIMATIC",17,1,"6AG40121CA210XX0"]
["6AG4012-1CB31-0BX0","SIMATIC IPC347E (RACK PC, 19\", 4U); CORE I5-4570S (4C/4T, 2.9 (3.6) GHZ, 6 MB CACHE); INTERFACES: 2X GBIT ETHERNET, 1X DVI-D, 1X VGA, 2X USB FRONT, 4X USB BACK, 1X USB INTERNAL, 2X SERIAL, 2X PS/2, AUDIO; 1X 1 TBYTE HDD, INTERNAL; 8 GBYTE DDR3 SDRAM (1X 8 GBYTE), SINGLE CHANNEL; DVD+/-RW; WINDOWS 7 ULT. 64 BIT SP1; 100/240 V INDUSTRIAL POWER SUPPLY, W/O POWER CORD;",2777,"ST",1,"SIMATIC",17,1,"6AG40121CB310BX0"]
["6AG4012-1CB31-0CX0","SIMATIC IPC347E (Rack PC, 19\", 4U); Core I5-4570S (4C/4T, 2.9 (3.6) GHz, 6 MB cache); Interfaces: 2x Gbit Ethernet, 1x DVI-D, 1x VGA, 2x USB on the front, 4x USB on the rear, 1x USB internal, 2x serial, 2x PS/2, audio; 1x 1TB HDD, internal; 8 GB DDR3 SD-RAM (1x 8 GB), single channel; DVD +/-RW; Windows 10 Enterprise LTSB 2016; 100/240V industryial power supply, without line cable",2549,"ST",1,"SIMATIC",17,1,"6AG40121CB310CX0"]
["6AG4012-1CE31-0BX0","SIMATIC IPC347E (RACK PC, 19\", 4U); CORE I5-4570S (4C/4T, 2.9 (3.6) GHZ, 6 MB CACHE); INTERFACES: 2X GBIT ETHERNET, 1X DVI-D, 1X VGA, 2X USB FRONT, 4X USB BACK, 1X USB INTERNAL, 2X SERIAL, 2X PS/2, AUDIO; 1X 256 BYTE SSD, INTERNAL; 8 GBYTE DDR3 SDRAM (1X 8 GBYTE), SINGLE CHANNEL; DVD+/-RW; WINDOWS 7 ULTIMATE 64 BIT SP1; 100/240 V INDUSTRIAL POWER SUPPLY,  W/O POWER CORD;",2939,"ST",1,"SIMATIC",17,1,"6AG40121CE310BX0"]
["6AG4012-1CE31-0CX0","SIMATIC IPC347E (Rack PC, 19\", 4U); core I5-4570S (4C/4T, 2.9 (3.6) GHz, 6 MB cache); interfaces: 2X Gbit Ethernet, 1X DVI-D, 1X VGA, 2X USB on the front, 4x USB on the rear, 1x USB internal, 2x serial, 2x PS/2, audio; 256G SSD, internal; 8 GB DDR3 SD-RAM (1x 8 GB), single channel; DVD +/-RW; Windows10 Enterprise LTSB 2016; 100/240V industrial power supply, without line cable",2711,"ST",1,"SIMATIC",17,1,"6AG40121CE310CX0"]
["6AG4021-0AA11-0AA0","SIMATIC IPC127E; Atom E3930 (2C/2T), 2 GB RAM; Base version; 2x Ethernet RJ45, 2x USB3.0; without operating system; 32 GB SSD; without mounting accessories",943,"ST",1,"SIMATIC",0.32,1,"6AG40210AA110AA0"]
["6AG4021-0AA11-1BA0","SIMATIC IPC127E; Atom E3930 (2C/2T), 2 GB RAM; Base version; 2x Ethernet RJ45, 2x USB3.0; Windows 10 Enterprise LTSB 2016, 64 bit, MUI (en, de, fr, it, es); 64 GB SSD; without mounting accessories",1299,"ST",1,"SIMATIC",0.32,1,"6AG40210AA111BA0"]
["6AG4021-0AA12-0BA0","SIMATIC IPC127E; Atom E3930 (2C/2T), 2 GB RAM; Extended version 3x Ethernet RJ45, 4x USB3.0; without operating system; 64 GB SSD; without mounting accessories",1202,"ST",1,"SIMATIC",0.4,1,"6AG40210AA120BA0"]
["6AG4021-0AA20-0AA1","SIMATIC IPC, Mounting kit DIN Rail for SIMATIC IPC127E",10.5,"ST",1,"SIMATIC",0.1,1,"6AG40210AA200AA1"]
["6AG4021-0AA20-0AA2","SIMATIC IPC, Mounting kit Wall mount for SIMATIC IPC127E",10.5,"ST",1,"SIMATIC",0.1,1,"6AG40210AA200AA2"]
["6AG4021-0AA20-0AA3","SIMATIC IPC, Mounting kit book mounting Base version for SIMATIC IPC127E",10.5,"ST",1,"SIMATIC",0.1,1,"6AG40210AA200AA3"]
["6AG4021-0AA20-0AA4","SIMATIC IPC, Mounting kit book mounting Extended version for SIMATIC IPC127E",10.5,"ST",1,"SIMATIC",0.1,1,"6AG40210AA200AA4"]
["6AG4021-0AA20-0AA5","SIMATIC IPC, Mounting kit book mounting DIN Rail for SIMATIC IPC127E",10.5,"ST",1,"SIMATIC",0.1,1,"6AG40210AA200AA5"]
["6AG4021-0AB11-0BA0","SIMATIC IPC127E; Atom E3940 (4C/4T), 4 GB RAM; Base version 2x Ethernet RJ45, 2x USB3.0; without operating system 64 GB SSD; without mounting accessories",1365,"ST",1,"SIMATIC",0.32,1,"6AG40210AB110BA0"]
["6AG4021-0AB11-1BA0","SIMATIC IPC127E; Atom E3940 (4C/4T), 4 GB RAM; Base version; 2x Ethernet RJ45, 2x USB3.0; Windows 10 Enterprise LTSB 2016, 64 bit, MUI (en, de, fr, it, es); 64 GB SSD; without mounting accessories",1592,"ST",1,"SIMATIC",0.32,1,"6AG40210AB111BA0"]
["6AG4021-0AB11-1CA0","SIMATIC IPC127E; Atom E3940 (4C/4T), 4 GB RAM; Base version; 2x Ethernet RJ45, 2x USB3.0; Windows 10 Enterprise LTSB 2016, 64 bit, MUI (en, de, fr, it, es); 128 GB SSD; without mounting accessories",1721,"ST",1,"SIMATIC",0.32,1,"6AG40210AB111CA0"]
["6AG4021-0AB12-0CA0","SIMATIC IPC127E; Atom E3940 (4C/4T), 4 GB RAM; Extended version 3x Ethernet RJ45, 4x USB3.0; without operating system 128 GB SSD; without mounting accessories",1624,"ST",1,"SIMATIC",0.4,1,"6AG40210AB120CA0"]
["6AG4021-0AB12-1BA0","SIMATIC IPC127E; Atom E3940 (4C/4T), 4 GB RAM; Extended version; 3x Ethernet RJ45, 4x USB3.0; Windows 10 Enterprise LTSB 2016, 64 bit, MUI (en, de, fr, it, es); 64 GB SSD; without mounting accessories",1721,"ST",1,"SIMATIC",0.4,1,"6AG40210AB121BA0"]
["6AG4021-0AB12-1CA0","SIMATIC IPC127E; Atom E3940 (4C/4T), 4 GB RAM; Extended version; 3x Ethernet RJ45, 4x USB3.0; Windows 10 Enterprise LTSB 2016, 64 bit, MUI (en, de, fr, it, es); 128 GB SSD; without mounting accessories",1852,"ST",1,"SIMATIC",0.4,1,"6AG40210AB121CA0"]
["6AG4022-0AA21-0BA1","SIMATIC IPC327E (BASICBOX PC); CELERON N3160 (4C/4T); 4 GB RAM; 500 GB HDD; 1x DISPLAY-PORT GRAPHIC; 1x VGA-PORT GRAPHIC; 2x 10/100/1000 MBIT/S ETHERNET RJ45; 2x USB3.0, 4x USB2.0; 6x COM-PORTS; 1x mPCIe-SLOT; 1x mSATA-SLOT; W/O OPERATING SYSTEM; 24V DC POWER SUPPLY; WALL MOUNTING, MOUNTING ON DIN RAIL",1185,"ST",1,"SIMATIC",2,1,"6AG40220AA210BA1"]
["6AG4022-0AA21-0CA1","SIMATIC IPC327E (Basicbox PC); Celeron N3160 (4C/4T); 4 GB RAM; 256 GB SSD; 1x Display-Port graphic; 1x VGA-Port graphic;2x 10/100/1000 MBit/s Ethernet RJ45; 2x USB3.0, 4x USB2.0; 6x serial Ports (COM); 1x mPCIe-Slot; 1x mSATA-Slot; w/o Operating system; DC 24V power supply; mounting on DIN rail; wall mounting,",1376,"ST",1,"SIMATIC",2,1,"6AG40220AA210CA1"]
["6AG4022-0AA21-1BA1","SIMATIC IPC327E (BASICBOX PC); CELERON N3160 (4C/4T); 4 GB RAM; 500 GB HDD; 1x DISPLAY-PORT GRAPHIC; 1x VGA-PORT GRAPHIC; 2x 10/100/1000 MBIT/S ETHERNET RJ45; 2x USB3.0, 4x USB2.0; 6x COM-PORTS; 1x mPCIe-SLOT; 1x mSATA-SLOT; WINDOWS 7 ULTIMATE SP1 64 Bit; 24V DC POWER SUPPLY; WALL MOUNTING, MOUNTING ON DIN RAIL",1694,"ST",1,"SIMATIC",2,1,"6AG40220AA211BA1"]
["6AG4022-0AA21-1CA1","SIMATIC IPC327E (Basicbox PC); Celeron N3160 (4C/4T); 4 GB RAM; 256 GB SSD; 1x Display-Port graphic; 1x VGA-Port graphic;2x 10/100/1000 MBit/s Ethernet RJ45; 2x USB3.0, 4x USB2.0; 6x serial Ports (COM); 1x mPCIe-Slot; 1x mSATA-Slot; Windows 7 Ultimate SP1 64 bit; DC 24V power supply; mounting on DIN rail; wall mounting,",1885,"ST",1,"SIMATIC",2,1,"6AG40220AA211CA1"]
["6AG4022-0AA21-2CA1","SIMATIC IPC327E (BASICBOX PC); Celeron N3160 (4C/4T); 4 GB RAM; 256 GB SSD; 1x DisplayPort Graphic; 1x VGA-Port Graphic; 2 x 10/100/1000 MBit/s Ethernet RJ45; 2x USB3.0, 4x USB2.0; 6x serial Ports (COM) 1x mPCIe / 1x mSATA; 1x mPCIe / 1x mSATA; Windows 10 Enterprise 2016 LTSB, 64 bit, MUI (en,de,fr,it,es); 24 V DC power supply; DIN rail, wall mounting;",1599,"ST",1,"SIMATIC",2.7,1,"6AG40220AA212CA1"]
["6AG4025-0AB10-0BB0","SIMATIC IPC527G, (Box PC); Pentium G4400 (2C/2T, 3.3 GHz); 1 TB HDD, internal; 4 GB DDR4; without operating system; 2x Gigabit Ethernet (IE/PN); 1x DisplayPort, 1x VGA; 4x USB 3.0, 2x USB 2.0; 2x RS232/485/422 (can be selected); 2x RS232, 1x 8 bit DIO, 2x PCI; 1x PCIe x16, 1x PCIe x1; 100/240 V AC power supply without line cable",1608,"ST",1,"SIMATIC",5,1,"6AG40250AB100BB0"]
["6AG4025-0CB20-0BB0","SIMATIC IPC527G (Box PC); Core i5-6500 (4C/4T, 3.2 (3.6) GHz); 1 TB HDD, internal; 8 GB DDR4; without operating system; 2x Gigabit Ethernet (IE/PN); 1x DisplayPort, 1x VGA; 4x USB 3.0, 2x USB 2.0; 2x RS232/485/422 (can be selected); 2x RS232, 1x 8 bit DIO, 2x PCI; 1x PCIe x16, 1x PCIe x1; 100/240 V AC power supply without line cable",2205,"ST",1,"SIMATIC",5,1,"6AG40250CB200BB0"]
["6AG4025-0CB20-2BB0","SIMATIC IPC527G (Box PC); Core i5-6500 (4C/4T, 3.2 (3.6) GHz); 1 TB HDD, internal; 8 GB DDR4; Windows 7 Ultimate 64-bit, MUI; 2x Gigabit Ethernet (IE/PN); 1x DisplayPort, 1x VGA; 4x USB 3.0, 2x USB 2.0; 2x RS232/485/422 (can be selected); 2x RS232, 1x 8 bit DIO, 2x PCI; 1x PCIe x16, 1x PCIe x1; 100/240 V AC power supply without line cable",2715,"ST",1,"SIMATIC",5,1,"6AG40250CB202BB0"]
["6AG4025-0CD20-0BB0","SIMATIC IPC527G (Box PC); Core i5-6500 (4C/4T, 3.2 (3.6) GHz); 128 GB SSD, internal; 8 GB DDR4; without operating system; 2x Gigabit Ethernet (IE/PN); 1x DisplayPort, 1x VGA; 4x USB 3.0, 2x USB 2.0; 2x RS232/485/422 (can be selected); 2x RS232, 1x 8 bit DIO, 2x PCI; 1x PCIe x16, 1x PCIe x1; 100/240 V AC power supply without line cable",2205,"ST",1,"SIMATIC",5,1,"6AG40250CD200BB0"]
["6AG4025-0CD20-2BB0","SIMATIC IPC527G (Box PC); Core i5-6500 (4C/4T, 3.2 (3.6) GHz); 128 GB SSD, internal; 8 GB DDR4; Windows 7 Ultimate 64-bit, MUI; 2x Gigabit Ethernet (IE/PN); 1x DisplayPort, 1x VGA; 4x USB 3.0, 2x USB 2.0; 2x RS232/485/422 (can be selected); 2x RS232, 1x 8 bit DIO, 2x PCI; 1x PCIe x16, 1x PCIe x1; 100/240 V AC power supply without line cable",2715,"ST",1,"SIMATIC",5,1,"6AG40250CD202BB0"]
["6AG4025-0CE20-2BB0","SIMATIC IPC527G (Box PC); Core i5-6500 (4C/4T, 3.2 (3.6) GHz); 256 GB SSD, internal; 8 GB DDR4; Windows 7 Ultimate 64-bit, MUI; 2x Gigabit Ethernet (IE/PN); 1x DisplayPort, 1x VGA; 4x USB 3.0, 2x USB 2.0; 2x RS232/485/422 (can be selected); 2x RS232, 1x 8 bit DIO, 2x PCI; 1x PCIe x16, 1x PCIe x1; 100/240 V AC power supply without line cable",2906,"ST",1,"SIMATIC",5,1,"6AG40250CE202BB0"]
["6AG4025-0CE20-3BB0","SIMATIC IPC527G (Box PC); Core i5-6500 (4C/4T, 3.2 (3.6) GHz); 256 GB SSD, internal; 8 GB DDR4; Windows 10 Enterprise 2016 LTSB 2x Gigabit Ethernet (IE/PN); 1x DisplayPort, 1x VGA; 4x USB 3.0, 2x USB 2.0; 2x RS232/485/422 (can be selected); 2x RS232, 1x 8 bit DIO, 2x PCI; 1x PCIe x16, 1x PCIe x1; 100/240 V AC power supply without line cable",2683,"ST",1,"SIMATIC",5,1,"6AG40250CE203BB0"]
["6AG4025-0DF20-2BB0","SIMATIC IPC527G (Box PC), Core i7-6700 (4C/8T, 3.4 (4.0) GHz); 512 GB SSD, internal; 8 GB DDR4; Windows 7 Ultimate 64 bit, MUI; 2x Gigabit Ethernet (IE/PN); 1x DisplayPort, 1x VGA; 4x USB3.0, 2x USB2.0; 2x RS232/485/422 (switchable); 2x RS232, 1x 8bit DIO, 2x PCI; 1x PCIe x16, 1x PCIe x1; 100/240V AC power supply without line cable",3542,"ST",1,"SIMATIC",5,1,"6AG40250DF202BB0"]
["6AG4025-0DF20-4BB0","SIMATIC IPC527G (Box PC), Core i7-6700 (4C/8T, 3.4 (4.0) GHz); 512 GB SSD, internal; 8 GB DDR4; Windows 10 Enterprise 2016 LTSB 2x Gigabit Ethernet (IE/PN); 1x DisplayPort, 1x VGA; 4x USB3.0, 2x USB2.0; 2x RS232/485/422 (switchable); 2x RS232, 1x 8bit DIO, 2x PCI; 1x PCIe x16, 1x PCIe x1; 100/240V AC power supply without line cable",3463,"ST",1,"SIMATIC",5,1,"6AG40250DF204BB0"]
["6AG4104-4AA05-3XX0","SIMATIC IPC547G (Rack PC, 19\", 4HU); Pentium Dual Core G4400 (2C/2T, 3.3 GHz, 3 MB cache); MB (chipset H110, 2x Gbit LAN, 2x USB 3.0 front, 2x USB 3.0 & 4x USB 2.0 on rear, 2x PS/2, audio; 1x display port V1.2, 1x DVI-D, 7 slots: 5x PCI-E, 2x PCI) 1x 1 TB HDD, internal; 4 GB DDR4 SD-RAM (1x 4 GB) Enclosure painted, COM2+LPT, 100/240V AC industrial power supply unit, without line cable; without operating system",1701,"ST",1,"SIMATIC",17,1,"6AG41044AA053XX0"]
["6AG4104-4GN16-4BX0","SIMATIC IPC547G (Rack PC, 19\", 4HU); Core i5-6500 (4C/4T, 3.2(3.6) GHz, 6 MB cache, iAMT); MB (CHIPSET C236, 2x Gbit LAN, 2x USB3.0 front, 4x USB3.0 & 4x USB2.0 rear, 1x USB2.0 int. 1x COM 1, 2x PS/2, audio; 2x display ports V1.2, 1x DVI-D, 7 slots: 5x PCI-E, 2x PCI) RAID1 2x 1 TB HDD in interchangeable insert, front; 8 GB DDR4 SD-RAM (2x 4 GB) Enclosure painted, COM2+LPT, DVD +/-RW (SLIM); Adapter cable DP acc. to VGA; 100/240V AC industrial power supply unit, without line cable; Windows 7 Ultimate 64 bit SP1",3077,"ST",1,"SIMATIC",18,1,"6AG41044GN164BX0"]
["6AG4104-4HP18-5BX0","SIMATIC IPC547G (Rack PC, 19\", 4HU); Core i7-6700 (4C/8T, 3.4(4.0) GHz, 8 MB cache, iAMT); MB (CHIPSET C236, 2x Gbit LAN, 2x USB 3.0 front, 4x USB 3.0 & 4x USB2.0 rear, 1x USB2.0 int. 1x COM 1, 2x PS/2, audio; 2x display ports V1.2, 1x DVI-D, 7 slots: 5x PCI-E, 2x PCI) RAID1 2x 1 TB HDD Enterprise in interchangeable insert, front; 8 GB DDR4 SD-RAM (2x 4 GB) Enclosure painted, COM2+LPT, DVD +/-RW (SLIM); Graphics card (DH: 2x DVI/VGA); 2x 100/240V redundant industrial power supply unit; without line cable; Windows 7 Ultimate 64 bit SP1",4242,"ST",1,"SIMATIC",19,1,"6AG41044HP185BX0"]
["6AG4141-1AA14-0FA0","SIMATIC IPC427E (Microbox PC); HD graphic onboard, 4x USB V3.0 (high current); PCIE (optional); Celeron G3902E; 3x Gbit Ethernet (IE/PN); w/o mounting accessories; working memory 4GB; w/o RS232/485; 1x PCIe (x4); Windows 7 Ultimate SP1, 64 Bit, MUI (ge, en, es, fr, it); w/o replaceable mass storage; Internal mass storage: 240 GB Solid-State Drive SATA; w/o SIMATIC Software; 24 V DC industrial power supply",2187,"ST",1,"SIMATIC",3,1,"6AG41411AA140FA0"]
["6AG4141-1AA17-0FA0","SIMATIC IPC427E (Microbox PC); HD graphic onboard, 4x USB V3.0 (high current); PCIE (optional); Celeron G3902E; 3x Gbit Ethernet (IE/PN); w/o mounting accessories; working memory 4GB; w/o RS232/485; 1x PCIe (x4); Windows 10 IoT Enterprise 2016 LTSB (64Bit) f. Celeron, I3/I5; w/o replaceable mass storage; Internal mass storage: 240 GB Solid-State Drive SATA; w/o SIMATIC Software; 24 V DC industrial power supply",2040,"ST",1,"SIMATIC",3,1,"6AG41411AA170FA0"]
["6AG4141-5AB14-0FA0","SIMATIC IPC427E (Microbox PC); HD graphic onboard, 4x USB V3.0 (high current); PCIE (optional); Core i5-6442EQ; 3x Gbit Ethernet (IE/PN); w/o mounting accessories; working memory 8GB; w/o RS232/485; 1x PCIe (x4); Windows 7 Ultimate SP1, 64 Bit, MUI (ge, en, es, fr, it); w/o replaceable mass storage; Internal mass storage: 240 GB Solid-State Drive SATA; w/o SIMATIC Software; 24 V DC industrial power supply",2859,"ST",1,"SIMATIC",3,1,"6AG41415AB140FA0"]
["6AG4141-5AB17-0FA0","SIMATIC IPC427E (Microbox PC); HD graphic onboard, 4x USB V3.0 (high current); PCIE (optional); Core i5-6442EQ; 3x Gbit Ethernet (IE/PN); w/o mounting accessories; working memory 8GB; w/o RS232/485; 1x PCIe (x4); Windows 10 IoT Enterprise 2016 LTSB (64Bit) f. Celeron, I3/I5; w/o replaceable mass storage; Internal mass storage: 240 GB Solid-State Drive SATA; w/o SIMATIC Software; 24 V DC industrial power supply",2712,"ST",1,"SIMATIC",3,1,"6AG41415AB170FA0"]
["6AG6003-0CF00-0AA0","SIPLUS RIC library for SIMATIC Software Controller consisting of - CD (software, Documentation). - Runtime license",1313,"ST",1,"SIMATIC",9.5000000000000001E-2,1,"6AG60030CF000AA0"]
["6AG6003-1CF00-0CA0","SIPLUS RIC library for SIMATIC S7-3xx consisting of - SIMATIC MMC 512 KB - CD (software, Documentation). - Runtime license",1407,"ST",1,"SIMATIC",0.125,1,"6AG60031CF000CA0"]
["6AG6003-1CF00-0DA0","SIPLUS RIC library for SIMATIC S7-3xx consisting of SIMATIC MMC 2 MB - CD (software, Documentation). - Runtime license",2142,"ST",1,"SIMATIC",0.125,1,"6AG60031CF000DA0"]
["6AG6003-3CF00-0AA0","SIPLUS RIC library for SIMATIC S7-4xx consisting of - CD (software,Documentation). - Runtime license for 1 CPU",1932,"ST",1,"SIMATIC",9.5000000000000001E-2,1,"6AG60033CF000AA0"]
["6AG6003-5CF00-0CA0","SIPLUS RIC library for SIMATIC ET 200S consisting of - SIMATIC MMC 512 KB - CD (software, Documentation). - Runtime license",813,"ST",1,"SIMATIC",0.125,1,"6AG60035CF000CA0"]
["6AG6003-5CF00-0DA0","SIPLUS RIC library for SIMATIC ET 200S consisting of - SIMATIC MMC 2 MB - CD (software, Documentation). - Runtime license",1155,"ST",1,"SIMATIC",0.125,1,"6AG60035CF000DA0"]
["6AG6003-7CF00-0LF0","SIPLUS RIC library for SIMATIC S7-1500/ET200SP consisting of SIMATIC SMC 24MB - CD (software, Documentation). - Runtime license",2016,"ST",1,"SIMATIC",0.125,1,"6AG60037CF000LF0"]
["6AG6003-7CF00-0LL0","SIPLUS RIC library for SIMATIC S7-1500/ET200SP consisting of SIMATIC SMC 256MB - CD (software, Documentation). - Runtime license",2153,"ST",1,"SIMATIC",0.125,1,"6AG60037CF000LL0"]
["6AG6003-7CF00-0LP0","SIPLUS RIC library for SIMATIC S7-1500/ET200SP consisting of SIMATIC SMC 2GB - CD (software and documentation - Runtime license",2720,"ST",1,"SIMATIC",0.125,1,"6AG60037CF000LP0"]
["6AG6003-8CF00-0LE0","SIPLUS RIC library for SIMATIC S7-1500/ET200SP consisting of SIMATIC SMC 12MB - CD (software, Documentation). - Runtime license",800,"ST",1,"SIMATIC",0.125,1,"6AG60038CF000LE0"]
["6AT8000-1BB00-0XA0","SIPLUS CMS-Hardware IFN ANALOG INPUT Acquisition of analog signals \"6*ADC; +/-10V; 192kHz; IP67\"",2625,"ST",1,"SIMATIC",0.8,1,"6AT80001BB000XA0"]
["6AT8000-1BB00-2XA0","SIPLUS CMS-Hardware IFN ANALOG INPUT distance Acquisition of analog signals \"6*ADC; +/-20V; 192kHz; IP67\"",2625,"ST",1,"SIMATIC",1.4,1,"6AT80001BB002XA0"]
["6AT8000-1BB00-4XA0","SIPLUS CMS-Hardware \"IFN VIB-A;\" \"Acquisition of analog signals;\" \"VIBRATION DETECTION 6*IEPE;\" for VIBRATION ACCELERATION \"measurement; UW=24 V DC; IP67\"",2625,"ST",1,"SIMATIC",1.5,1,"6AT80001BB004XA0"]
["6AT8000-1EA00-1XA0","SIPLUS CMS-Hardware RPN \"IEEE 1394B T002; IEEE 1394B\" \"Multi-port repeater; 2 opt.\" \"and 1 electr. interface;\" UW=24 V DC",2373,"ST",1,"SIMATIC",0.5,1,"6AT80001EA001XA0"]
["6AT8000-1EB00-3XA0","SIPLUS CMS-Hardware MCN11 \"Media converter node;\" 1 opt. and 1 electr. \"interfaces;\" \"UW=24 V DC; IP67\"",2415,"ST",1,"SIMATIC",0.6,1,"6AT80001EB003XA0"]
["6AT8000-2AA00-1AA3","SIPLUS CMS accessories Cable-IEEE1394A-66-0030 \"Length=00.30 m; 6-6 connector\"",24.6,"ST",1,"SIMATIC",2.5000000000000001E-2,1,"6AT80002AA001AA3"]
["6AT8000-2AA00-1AC0","SIPLUS CMS accessories Cable-IEEE1394A-66-0200 \"Length=02.00 m; 6-6 connector\"",34.200000000000003,"ST",1,"SIMATIC",2.5000000000000001E-2,1,"6AT80002AA001AC0"]
["6AT8000-2AA00-1AE5","SIPLUS CMS accessories Cable-IEEE1394A-66-0450 \"Length=04.50 m; 6-6 connector\"",37.300000000000004,"ST",1,"SIMATIC",2.5000000000000001E-2,1,"6AT80002AA001AE5"]
["6AT8000-2AB20-1AB0","SIPLUS CMS accessories Cable-IEEE1394A-8F-0040 \"Length=0.40 m;\" IEEE1394 IFN-PC coupling",118,"ST",1,"SIMATIC",0.04,1,"6AT80002AB201AB0"]
["6AT8000-2AB20-1AC0","SIPLUS CMS accessories Cable-IEEE1394A-8F-0200 \"Length=2.00 m;\" IEEE1394 IFN-PC coupling",120,"ST",1,"SIMATIC",0.12,1,"6AT80002AB201AC0"]
["6AT8000-2AB20-1AE5","SIPLUS CMS accessories Cable-IEEE1394A-8F-0450 \"Length=4.50 m;\" IEEE1394 IFN-PC coupling",121,"ST",1,"SIMATIC",0.24,1,"6AT80002AB201AE5"]
["6AT8000-2AB20-2AA2","SIPLUS CMS accessories Cable-IEEE1394A-8m-0030 \"Length = 0.30 m;\" IEEE1394 IFN-MCN11 coupling",122,"ST",1,"SIMATIC",0.06,1,"6AT80002AB202AA2"]
["6AT8000-2AB20-2AD2","SIPLUS CMS accessories Cable-IEEE1394A-88-0020 \"Length = 0.20 m;\" IEEE1394 IFN-IFN coupling",123,"ST",1,"SIMATIC",0.04,1,"6AT80002AB202AD2"]
["6AT8000-2AB30-1AA1","SIPLUS CMS accessories \"Cable-Power-135-0000;\" \"Length=1.35 m;\" IFN power cable",18.100000000000001,"ST",1,"SIMATIC",0.1,1,"6AT80002AB301AA1"]
["6AT8000-2AB30-1AA2","SIPLUS CMS accessories \"Cable-Power-200-0000;\" \"Length=2.00 m;\" IFN power cable",23.3,"ST",1,"SIMATIC",0.12,1,"6AT80002AB301AA2"]
["6AT8000-2AB30-1AA5","SIPLUS CMS accessories \"Cable-Power-500-0000;\" \"Length=5.00 m;\" IFN power cable",26.900000000000002,"ST",1,"SIMATIC",0.28000000000000003,1,"6AT80002AB301AA5"]
["6AT8000-2AB30-1AB0","SIPLUS CMS accessories \"Cable-Power-1000-0000;\" \"Length=10.00 m;\" IFN power cable",32.200000000000003,"ST",1,"SIMATIC",0.52,1,"6AT80002AB301AB0"]
["6AT8000-2AB40-1AA2","SIPLUS CMS accessories \"Cable-IO-200-0000;\" \"Length=2.00 m;\" IFN IO cable",19.5,"ST",1,"SIMATIC",0.12,1,"6AT80002AB401AA2"]
["6AT8000-2AB40-1AA5","SIPLUS CMS accessories \"Cable-IO-500-0000;\" \"Length=5.00 m;\" IFN IO cable",26.900000000000002,"ST",1,"SIMATIC",0.28000000000000003,1,"6AT80002AB401AA5"]
["6AT8000-2AB40-1AB0","SIPLUS CMS accessories \"Cable-IO-1000-0000;\" \"Length=10.00 m;\" IFN IO cable",32.200000000000003,"ST",1,"SIMATIC",0.52,1,"6AT80002AB401AB0"]
["6AT8000-2AB50-1AA2","SIPLUS CMS- \"Accessory IFN ADD0020;\" \"Length = 0.20 m;\" IFN energy and IEEE1394 cable",120,"ST",1,"SIMATIC",0.12,1,"6AT80002AB501AA2"]
["6AT8000-2AB50-1AB0","SIPLUS CMS- \"Accessory IFN ADD0100;\" \"Length=1.00 m;\" IFN energy and IEEE1394 cable",124,"ST",1,"SIMATIC",0.2,1,"6AT80002AB501AB0"]
["6AT8000-2AB50-1AC0","SIPLUS CMS- \"Accessory IFN ADD0200;\" \"Length=2.00 m;\" IFN energy and IEEE1394 cable",131,"ST",1,"SIMATIC",0.28000000000000003,1,"6AT80002AB501AC0"]
["6AT8000-2AB50-1AE5","SIPLUS CMS- \"Accessory IFN ADD0450;\" \"Length=4.50 m;\" IFN energy and IEEE1394 cable",158,"ST",1,"SIMATIC",0.52,1,"6AT80002AB501AE5"]
["6AT8000-2BB00-0XA0","SIPLUS CMS- Accessory set of caps for IFN AI and IFN VIB-A",15.5,"ST",1,"SIMATIC",0.2,1,"6AT80002BB000XA0"]
["6AT8000-2BB00-0XB0","SIPLUS CMS- \"Accessories mounting kit;\" Wall holder for IFN AI and IFN VIB-A",21.900000000000002,"ST",1,"SIMATIC",0.04,1,"6AT80002BB000XB0"]
["6AT8000-2BB00-0XC0","SIPLUS CMS- \"Accessories mounting kit;\" Wall holder for MCN11",26.900000000000002,"ST",1,"SIMATIC",0.04,1,"6AT80002BB000XC0"]
["6AT8002-1AA00","SIPLUS CMS2000 basic unit \"VIB; 2 IEPE vibration channels; 2 analog inputs for \"Process value; 1 digital input \"for rotational speed acquisition;\" System and limit value messages via 3 digital outputs",1701,"ST",1,"SIMATIC",0.33,1,"6AT80021AA00"]
["6AT8002-2AA00","SIPLUS CMS2000 VIB-MUX 8 IEPE input channels in MULTIPLEX mode are switched to one output channel Control via the system interface max. 2 VIB-MUX modules per Basic Unit VIB can be used",812,"ST",1,"SIMATIC",0.33,1,"6AT80022AA00"]
["6AT8002-4AA00","SIPLUS CMS2000 shield support for the EMC-compliant Connection of signal and encoder cables to the basic unit VIB Packing unit with 2 units",92,"ST",1,"SIMATIC",0.28000000000000003,1,"6AT80024AA00"]
["6AT8002-4AB00","SIPLUS CMS2000 VIB-Sensor S01 \"Vibration sensor;\" Frequency range 0.5 Hz to \"15 kHz; measuring range 50G;\" sensitivity 100 mV/G \"(+/-10%); MIL connector top\"",320,"ST",1,"SIMATIC",9.7000000000000003E-2,1,"6AT80024AB00"]
["6AT8002-4AC03","SIPLUS CMS2000 cable MIL-300 Connecting cable for connection of VIB sensors with MIL connectors; Length=3.00 m",126,"ST",1,"SIMATIC",0.19,1,"6AT80024AC03"]
["6AT8002-4AC10","SIPLUS CMS2000 cable MIL-1000 Connecting cable for connection of VIB sensors with MIL connectors; Length=10.00 m",225,"ST",1,"SIMATIC",0.35199999999999998,1,"6AT80024AC10"]
["6AT8007-1AA10-0AA0","SIPLUS CMS1200 SM1281 Condition monitoring for SIMATIC S7-1200 \"4 IEPE vibration channels;\" 1 digital input for rotational speed acquisition",1103,"ST",1,"SIMATIC",0.28999999999999998,1,"6AT80071AA100AA0"]
["6AT8007-1AA20-0AA0","SIPLUS CMS1200 SM1281 \"Shield bracket set;\" for the EMC-compliant connection of cables to the SM1281 Packing unit with 2 units",55.300000000000004,"ST",1,"SIMATIC",0.13,1,"6AT80071AA200AA0"]
["6AV2100-0AA05-0AA5","SIMATIC WinCC Basic V15.1, Engineering Software in TIA Portal; Floating License; SW and documentation on DVD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (64-bit), Windows 10 (64-bit), WinSrv 2012 R2/2016 (64-bit) for configuration of SIMATIC Basic Panels ******************************* Content: Set (3x DVD + 1x USB)",116,"ST",1,"SIMATIC",0.251,1,"6AV21000AA050AA5"]
["6AV2100-0AA05-0AH5","SIMATIC WinCC Basic V15.1, Engineering software in TIA Portal; Floating License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (64 bit), Windows 10 (64 bit), WinSrv 2012 R2/2016 (64 bit) for configuration of SIMATIC Basic Panels ******************************* E-mail address required for delivery",104,"ST",1,"SIMATIC",1E-3,1,"6AV21000AA050AH5"]
["6AV2100-3AA05-0AE5","SIMATIC WinCC Basic V15.1, Upgrade V11..V14 -> V15.1; Engineering software in the TIA Portal; Floating license; SW and documentation on DVD; License key on a USB stick; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (64-bit), Windows 10 (64-bit), WinSrv 2012 R2/2016 (64-bit) for configuration of SIMATIC Basic Panels ******************************* Content: Set (5x DVD + 1x USB)",46.1,"ST",1,"SIMATIC",0.30599999999999999,1,"6AV21003AA050AE5"]
["6AV2100-3AA05-0AK5","SIMATIC WinCC Basic V15.1, Upgrade V11..V14 -> V15.1; Engineering software in TIA Portal; Floating License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (64 bit), Windows 10 (64 bit), WinSrv 2012 R2/2016 (64 bit) for configuration of SIMATIC Basic Panels ******************************* E-mail address required for delivery",42,"ST",1,"SIMATIC",1E-3,1,"6AV21003AA050AK5"]
["6AV2101-0AA00-0AQ0","EPL Royalty for SIMATIC WinCC Comfort, only valid in connection with Enterprise License contract, requires EPL Master",810,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21010AA000AQ0"]
["6AV2101-0AA00-0AR0","EPL Maintenance for SIMATIC WinCC Comfort, (EPL=Enterprise License) Payment for maintenance of a Royalty for 12 months, only valid in connection with Enterprise License contract, requires EPL Master",152,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21010AA000AR0"]
["6AV2101-0AA00-0UA0","SIMATIC WinCC Comfort V15.1 UCL package (TIA Portal) for one installation; Engineering software; Software and documentation on DVD; Master license on CD; UCL agreement required",649,"ST",1,"SIMATIC",0.28699999999999998,1,"6AV21010AA000UA0"]
["6AV2101-0AA00-0UH0","SIMATIC WinCC Comfort V15.1 UCL package (TIA Portal) for one installation; Engineering software; Software, documentation and master license for download; UCL agreement required ******************************* E-mail address required for delivery",587,"ST",1,"SIMATIC",1E-3,1,"6AV21010AA000UH0"]
["6AV2101-0AA05-0AA5","SIMATIC WinCC Comfort V15.1, Engineering software in TIA Portal; Floating License; SW and documentation on DVD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (64-bit), Windows 10 (64-bit), WinSrv 2012 R2/2016 (64-bit) for configuration of SIMATIC Panels ******************************* Content: Set (3x DVD + 1x USB)",830,"ST",1,"SIMATIC",0.26200000000000001,1,"6AV21010AA050AA5"]
["6AV2101-0AA05-0AH5","SIMATIC WinCC Comfort V15.1, Engineering software in TIA Portal; Floating License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (64 bit), Windows 10 (64 bit), WinSrv 2012 R2/2016 (64 bit) for configuration of SIMATIC Panels ******************************* E-mail address required for delivery",734,"ST",1,"SIMATIC",1E-3,1,"6AV21010AA050AH5"]
["6AV2101-2AA05-0BD5","SIMATIC WinCC Comfort Powerpack WinCC Basic-> WinCC Comfort V15 (without version change); engineering software in the TIA Portal; Floating License; Without software a. documentation; License key on USB flash drive; Class A; only valid for 6AV2100-0AA05-0AA5 or 6AV2100-0AA05-0AH5 ******************************* Content: 1x USB",713,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21012AA050BD5"]
["6AV2101-2AA05-0BJ5","SIMATIC WinCC Comfort Powerpack WinCC Basic-> WinCC Comfort V15 (without version replacement); Engineering software in the TIA Portal; Floating license; License key for download; without software a. documentation; Class A; only valid for 6AV2100-0AA05-0AA5 or 6AV2100-0AA05-0AH5 ******************************* E-mail address mandatory for delivery",630,"ST",1,"SIMATIC",1E-3,1,"6AV21012AA050BJ5"]
["6AV2101-3AA00-0UE0","SIMATIC WinCC Comfort V15.1 UCL (TIA Portal) Upgrade V11..V14 -> V15.1; for one installation; Engineering software; Software and documentation on DVD; Master license on CD; UCL agreement required",261,"ST",1,"SIMATIC",0.34200000000000003,1,"6AV21013AA000UE0"]
["6AV2101-3AA00-0UK0","SIMATIC WinCC Comfort V15.1 UCL (TIA Portal) Upgrade V11..V14 -> V15.1; for one installation; Engineering software; Software, documentation and master license for download; UCL agreement required ******************************* E-mail address required for delivery",236,"ST",1,"SIMATIC",1E-3,1,"6AV21013AA000UK0"]
["6AV2101-3AA05-0AE5","SIMATIC WinCC Comfort V15.1, Upgrade V11..V14 -> V15.1 or V11..V14 Combo-> V15.1 Combo; Engineering software in the TIA Portal; Floating license; SW and documentation on DVD; License key on a USB stick; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (64-bit), Windows 10 (64-bit), WinSrv 2012 R2/2016 (64-bit) for configuration of SIMATIC Panels ******************************* Content: Set (5x DVD + 1x USB)",331,"ST",1,"SIMATIC",0.317,1,"6AV21013AA050AE5"]
["6AV2101-3AA05-0AK5","SIMATIC WinCC Comfort V15.1, Upgrade V11..V14 -> V15.1 or V11..V14 Combo-> V15.1 Combo; Engineering software in TIA Portal; Floating License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (64 bit), Windows 10 (64 bit), WinSrv 2012 R2/2016 (64 bit) for configuration of SIMATIC Panels ******************************* E-mail address required for delivery",294,"ST",1,"SIMATIC",1E-3,1,"6AV21013AA050AK5"]
["6AV2101-4AB00-0UE0","SIMATIC WinCC Comfort V15.1 UCL (TIA Portal) Upgrade WinCC flexible 2008 Compact -> WinCC Comfort V15.1; for one installation; Engineering software; Software and documentation on DVD; Master license on CD; UCL agreement required",741,"ST",1,"SIMATIC",0.34200000000000003,1,"6AV21014AB000UE0"]
["6AV2101-4AB00-0UK0","SIMATIC WinCC Comfort V15.1 UCL (TIA Portal) Upgrade WinCC flexible 2008 Compact -> WinCC Comfort V15.1; for one installation; Engineering software; Software, documentation and master license for download; UCL agreement required ******************************* E-mail address required for delivery",672,"ST",1,"SIMATIC",1E-3,1,"6AV21014AB000UK0"]
["6AV2101-4AB05-0AE5","SIMATIC WinCC Comfort V15.1 upgrade WinCC flexible 2008 Compact-> WinCC Comfort V15.1 Combo; Engineering software in the TIA Portal; Floating license; SW and documentation on DVD; License key on a USB stick; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (64-bit), Windows 10 (64-bit), WinSrv 2012 R2/2016 (64-bit) for configuration of SIMATIC Panels ******************************* Content: Set (5x DVD + 1x USB)",945,"ST",1,"SIMATIC",0.317,1,"6AV21014AB050AE5"]
["6AV2101-4AB05-0AK5","SIMATIC WinCC Comfort V15.1, Upgrade WinCC flexible 2008 Compact-> WinCC Comfort V15.1 Combo; Engineering software in TIA Portal; Floating License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (64 bit), Windows 10 (64 bit), WinSrv 2012 R2/2016 (64 bit) for configuration of SIMATIC Panels ******************************* E-mail address required for delivery",840,"ST",1,"SIMATIC",1E-3,1,"6AV21014AB050AK5"]
["6AV2101-4BB00-0UE0","SIMATIC WinCC Comfort V15.1 UCL (TIA Portal) Upgrade WinCC flexible 2008 Standard -> WinCC Comfort V15.1; for one installation; Engineering software; Software and documentation on DVD; Master license on CD; UCL agreement required",261,"ST",1,"SIMATIC",0.34200000000000003,1,"6AV21014BB000UE0"]
["6AV2101-4BB00-0UK0","SIMATIC WinCC Comfort V15.1 UCL (TIA Portal) Upgrade WinCC flexible 2008 Standard -> WinCC Comfort V15.1; for one installation; Engineering software; Software, documentation and master license for download; UCL agreement required ******************************* E-mail address required for delivery",236,"ST",1,"SIMATIC",1E-3,1,"6AV21014BB000UK0"]
["6AV2101-4BB05-0AE5","SIMATIC WinCC Comfort V15.1 upgrade WinCC flexible 2008 Standard-> WinCC Comfort V15.1 Combo; Engineering software in the TIA Portal; Floating license; SW and documentation on DVD; License key on a USB stick; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (64-bit), Windows 10 (64-bit), WinSrv 2012 R2/2016 (64-bit) for configuration of SIMATIC Panels ******************************* Content: Set (5x DVD + 1x USB)",331,"ST",1,"SIMATIC",0.317,1,"6AV21014BB050AE5"]
["6AV2101-4BB05-0AK5","SIMATIC WinCC Comfort V15.1, Upgrade WinCC flexible 2008 Standard-> WinCC Comfort V15.1 Combo; Engineering software in TIA Portal; Floating License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (64 bit), Windows 10 (64 bit), WinSrv 2012 R2/2016 (64 bit) for configuration of SIMATIC Panels ******************************* E-mail address required for delivery",294,"ST",1,"SIMATIC",1E-3,1,"6AV21014BB050AK5"]
["6AV2102-0AA00-0AQ0","EPL Royalty for SIMATIC WinCC Advanced, only valid in connection with Enterprise License contract, requires EPL Master",2028,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21020AA000AQ0"]
["6AV2102-0AA00-0AR0","EPL Maintenance for SIMATIC WinCC Advanced, (EPL=Enterprise License) Payment for maintenance of a Royalty for 12 months, only valid in connection with Enterprise License contract, requires EPL Master",380,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21020AA000AR0"]
["6AV2102-0AA00-0UA0","SIMATIC WinCC Advanced V15.1 UCL package (TIA Portal) for one installation; Engineering software; Software and documentation on DVD; Master license on CD; UCL agreement required",1623,"ST",1,"SIMATIC",0.28699999999999998,1,"6AV21020AA000UA0"]
["6AV2102-0AA00-0UH0","SIMATIC WinCC Advanced V15.1 UCL package (TIA Portal) for one installation; Engineering software; Software, documentation and master license for download; UCL agreement required ******************************* E-mail address required for delivery",1470,"ST",1,"SIMATIC",1E-3,1,"6AV21020AA000UH0"]
["6AV2102-0AA05-0AA5","SIMATIC WinCC Advanced V15.1, Engineering software in TIA Portal; Floating License; SW and documentation on DVD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (64-bit), Windows 10 (64-bit), WinSrv 2012 R2/2016 (64-bit) for configuration of SIMATIC Panels, WinCC Runtime Advanced ******************************* Content: Set (3x DVD + 1x USB)",2069,"ST",1,"SIMATIC",0.26400000000000001,1,"6AV21020AA050AA5"]
["6AV2102-0AA05-0AA7","SIMATIC STEP 7 Basic/Prof., WinCC Basic/Comfort/Advanced Trial V15/15.1, Engineering Software in TIA Portal; Trial License; SW and documentation on DVD; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (64-bit), Windows 10 (64-bit), WinSrv 2012 R2/2016 (64-bit) for configuration of SIMATIC S7-1200/1500, SIMATIC S7-300/400/WinAC, SIMATIC Panels, WinCC Runtime Advanced ******************************* Content: Set (4x DVD)",27.900000000000002,"ST",1,"SIMATIC",0.24099999999999999,1,"6AV21020AA050AA7"]
["6AV2102-0AA05-0AH5","SIMATIC WinCC Advanced V15.1, Engineering software in TIA Portal; Floating License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (64 bit), Windows 10 (64 bit), WinSrv 2012 R2/2016 (64 bit) for configuration of SIMATIC Panels, WinCC Runtime Advanced ******************************* E-mail address required for delivery",1838,"ST",1,"SIMATIC",1E-3,1,"6AV21020AA050AH5"]
["6AV2102-0AA05-0AS5","SCE Trainer Package HMI WinCC Advanced V15 / WinCC flexible Advanced 2008 Content: SW and documentation on DVD, 6-unit license on USB stick, for WinCC Advanced V15/ WinCC flexible Advanced 2008 Engineering, Runtime, Options; 1x software for 20 students (6AV2102-0AA05-0AS7) for educational purposes only",812,"ST",1,"SIMATIC",1.333,1,"6AV21020AA050AS5"]
["6AV2102-0AA05-0AS7","SCE Trainer Package HMI WinCC Advanced V15/ WinCC flexible Advanced 2008, Software for 20 students for 365 days, Content: SW and documentation on DVD, 20 licenses for 365 days on USB flash drive, for WinCC Advanced V15/ WinCC flexible Advanced 2008 Engineering, Runtime; ******************************* for educational purposes only",245,"ST",1,"SIMATIC",0.50800000000000001,1,"6AV21020AA050AS7"]
["6AV2102-0AB05-0AS7","SCE Trainer Package HMI WinCC Advanced V15/ WinCC flexible Advanced 2008, software for 100 students for 365 days, Content: SW and documentation on DVD, 100 licenses for 365 days on USB flash drive, for WinCC Advanced V15/ WinCC flexible Advanced 2008 Engineering, Runtime; ******************************* for educational purposes only",245,"ST",1,"SIMATIC",1.149,1,"6AV21020AB050AS7"]
["6AV2102-0AC05-0AS7","SCE Trainer Project Package STEP 7/WinCC Advanced V15/ WinCC flexible Advanced 2008, Startdrive V15, SIMIT V9.1, STEP 7 Safety Advanced, PLCSIM / PLCSIM Advanced Software for 1 student for 365 days, Content: SW and documentation on DVD, license on USB stick for 365 days for STEP 7 Prof. V15, 2017/ STEP 7 Safety Advanced V15/5.4/ WinCC Advanced V15/ WinCC flexible Advanced 2008 Engineering, Runtime ******************************* for educational purposes only",55.6,"ST",1,"SIMATIC",0.95799999999999996,1,"6AV21020AC050AS7"]
["6AV2102-2AA00-0UC0","SIMATIC WinCC Advanced V15 UCL (TIA Portal) Powerpack WinCC Comfort V15 -> WinCC Advanced V15, for one installation; Engineering software; Master license on CD; UCL agreement required",973,"ST",1,"SIMATIC",0.17599999999999999,1,"6AV21022AA000UC0"]
["6AV2102-2AA00-0UJ0","SIMATIC WinCC Advanced V15 UCL (TIA Portal) Powerpack WinCC Comfort V15 -> WinCC Advanced V15, for one installation; Engineering software; master license for download; UCL agreement required ******************************* E-mail address required for delivery",882,"ST",1,"SIMATIC",1E-3,1,"6AV21022AA000UJ0"]
["6AV2102-2AA05-0BD5","SIMATIC WinCC Advanced Powerpack WinCC Comfort-> WinCC Advanced V15 (without version change); engineering software in the TIA Portal; Floating License; Without software a. documentation; License key on USB flash drive; Class A ******************************* Content: 1x USB",1239,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21022AA050BD5"]
["6AV2102-2AA05-0BJ5","SIMATIC WinCC Advanced Power Pack WinCC Comfort-> WinCC Advanced V15 (without version replacement); Engineering software in the TIA Portal; Floating License; License key for download; without software and documentation Class A ******************************* e-mail address required for delivery",1103,"ST",1,"SIMATIC",1E-3,1,"6AV21022AA050BJ5"]
["6AV2102-3AA00-0UE0","SIMATIC WinCC Advanced V15.1 UCL (TIA Portal) Upgr. V11..V14 -> V15.1; for one installation; Engineering software; Software and documentation on DVD; Master license on CD; UCL agreement required",648,"ST",1,"SIMATIC",0.34200000000000003,1,"6AV21023AA000UE0"]
["6AV2102-3AA00-0UK0","SIMATIC WinCC Advanced V15.1 UCL (TIA Portal) Upgrade V11..V14 -> V15.1; for one installation; Engineering software; Software, documentation and master license for download; UCL agreement required ******************************* E-mail address required for delivery",588,"ST",1,"SIMATIC",1E-3,1,"6AV21023AA000UK0"]
["6AV2102-3AA05-0AE5","SIMATIC WinCC Advanced V15.1, Upgrade V11..V14 -> V15.1 or V11..V14 Combo-> V15.1 Combo; Engineering software in the TIA Portal; Floating license; SW and documentation on DVD; License key on a USB stick; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (64-bit), Windows 10 (64-bit), WinSrv 2012 R2/2016 (64-bit) for configuration of SIMATIC Panels, WinCC Runtime Advanced ******************************* Content: Set (5x DVD + 1x USB)",830,"ST",1,"SIMATIC",0.317,1,"6AV21023AA050AE5"]
["6AV2102-3AA05-0AK5","SIMATIC WinCC Advanced V15.1, Upgrade V11..V14 -> V15.1 or V11..V14 Combo-> V15.1 Combo; Engineering software in TIA Portal; Floating License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (64 bit), Windows 10 (64 bit), WinSrv 2012 R2/2016 (64 bit) for configuration of SIMATIC Panels, WinCC RT Advanced ******************************* E-mail address required for delivery",735,"ST",1,"SIMATIC",1E-3,1,"6AV21023AA050AK5"]
["6AV2102-4AA00-0UE0","SIMATIC WinCC Advanced V15.1 UCL (TIA Portal) Upgrade WinCC flexible 2008 Advanced -> WinCC Advanced V15; for one installation; Engineering software; Software and documentation on DVD; Master license on CD; UCL agreement required",648,"ST",1,"SIMATIC",0.34200000000000003,1,"6AV21024AA000UE0"]
["6AV2102-4AA00-0UK0","SIMATIC WinCC Advanced V15.1 UCL (TIA Portal) Upgrade WinCC flexible 2008 Advanced -> WinCC Advanced V15.1; for one installation; Engineering software; Software, documentation and master license for download; UCL agreement required ******************************* E-mail address required for delivery",588,"ST",1,"SIMATIC",1E-3,1,"6AV21024AA000UK0"]
["6AV2102-4AA05-0AE5","SIMATIC WinCC Advanced V15.1 upgrade WinCC flexible 2008 Advanced-> WinCC Advanced V15.1 Combo; Engineering software in the TIA Portal; Floating license; SW and documentation on DVD; License key on a USB stick; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (64-bit), Windows 10 (64-bit), WinSrv 2012 R2/2016 (64-bit) for configuration of SIMATIC Panels, WinCC Runtime Advanced ******************************* Content: Set (5x DVD + 1x USB)",830,"ST",1,"SIMATIC",0.317,1,"6AV21024AA050AE5"]
["6AV2102-4AA05-0AK5","SIMATIC WinCC Advanced V15.1, Upgrade WinCC flexible 2008 Advanced-> WinCC Advanced V15.1 Combo; Engineering software in TIA Portal; Floating License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (64 bit), Windows 10 (64 bit), WinSrv 2012 R2/2016 (64 bit) for configuration of SIMATIC Panels, WinCC RT Advanced ******************************* E-mail address required for delivery",735,"ST",1,"SIMATIC",1E-3,1,"6AV21024AA050AK5"]
["6AV2102-4AA05-0AS5","SCE Trainer Package HMI Upgrade WinCC Advanced V15 / WinCC flexible Advanced 2008 Content: SW and documentation on DVD, 6-unit license on USB stick, for WinCC Advanced V15/ WinCC flexible Advanced 2008 Engineering, Runtime, Options; for educational purposes only",327,"ST",1,"SIMATIC",0.65800000000000003,1,"6AV21024AA050AS5"]
["6AV2103-0AA05-0AA7","SIMATIC STEP 7 Professional, WinCC Prof. Trial V15/V15.1, Engineering Software in TIA Portal; Trial License; SW and documentation on DVD; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (64-bit), Windows 10 (64-bit), WinSrv 2012 R2/2016 (64-bit) for configuration of SIMATIC Panels, SIMATIC S7-1200/1500, SIMATIC S7-300/400/WinAC, WinCC Runtime Advanced, WinCC Runtime Professional ******************************* Content: Set (4x DVD)",27.900000000000002,"ST",1,"SIMATIC",0.24099999999999999,1,"6AV21030AA050AA7"]
["6AV2103-0DA00-0AL0","SIMATIC WinCC Professional 512 Power Tags, SUS Software Update Service, within the framework of this contract, you will receive for one year all up-to-date software versions, the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software",441,"ST",1,"SIMATIC",1.2E-2,1,"6AV21030DA000AL0"]
["6AV2103-0DA00-0AM0","SIMATIC WinCC Professional 512 Power Tags, SUS (Compact) Software Update Service, for multiple orders on one position, these deliveries are grouped. Minimum order quantity: 3 units within the framework of this contract, you will receive for one year all up-to-date software versions, the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software",441,"ST",1,"SIMATIC",1.2E-2,1,"6AV21030DA000AM0"]
["6AV2103-0DA00-0AQ0","EPL Royalty for SIMATIC WinCC Professional 512 Power Tags, only valid in connection with Enterprise License contract, requires EPL Master",2317,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21030DA000AQ0"]
["6AV2103-0DA00-0AR0","EPL Maintenance for SIMATIC WinCC Professional 512 Power Tags, (EPL=Enterprise License) Payment for maintenance of a Royalty for 12 months, only valid in connection with Enterprise License contract, requires EPL Master",433,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21030DA000AR0"]
["6AV2103-0DA00-0AY0","SIMATIC WinCC Professional 512 Power Tags, SUS (download), Software Update Service, within the framework of this contract, you will receive for one year all up-to-date software versions, the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software ******************************* E-mail address required for delivery",412,"ST",1,"SIMATIC",1E-3,1,"6AV21030DA000AY0"]
["6AV2103-0DA00-0UA0","SIMATIC WinCC Professional 512 PowerTags V15.1; UCL package (TIA Portal) for one installation; Engineering software; Software and documentation on DVD; Master license on CD; UCL agreement required",1854,"ST",1,"SIMATIC",0.28699999999999998,1,"6AV21030DA000UA0"]
["6AV2103-0DA00-0UH0","SIMATIC WinCC Professional 512 PowerTags V15.1 UCL package (TIA Portal) for one installation; Engineering software; Software, documentation and master license for download; UCL agreement required ******************************* E-mail address required for delivery",1680,"ST",1,"SIMATIC",1E-3,1,"6AV21030DA000UH0"]
["6AV2103-0DA00-0UL0","SIMATIC WinCC Professional 512 Power Tags, SUS (UCL) Software Update Service, Automatic subsequent deliveries of upgrades and service packs for one year with automatic extension, requires current software version, only valid in connection with Unlock Copy License agreement Minimum ordering quantity 20 units",353,"ST",1,"SIMATIC",1.2E-2,1,"6AV21030DA000UL0"]
["6AV2103-0DA00-0UY0","SIMATIC WinCC Professional 512 Power Tags, SUS (UCL download) Software Update Service, Automatic subsequent deliveries of Upgrades and service packs for one year with automatic extension; requires current software version; only valid in connection with Unlock Copy License agreement; Minimum ordering quantity 20 units ******************************* E-mail address required for delivery",330,"ST",1,"SIMATIC",1E-3,1,"6AV21030DA000UY0"]
["6AV2103-0DA05-0AA5","SIMATIC WinCC Professional 512 PowerTags V15.1, Engineering software in TIA Portal; Floating License; SW and documentation on DVD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (64-bit), Windows 10 (64-bit), WinSrv 2012 R2/2016 (64-bit) for configuration of SIMATIC Panels, WinCC Runtime Advanced, WinCC Runtime Professional (512 PowerTags) ******************************* Content: Set (3x DVD + 1x USB)",2363,"ST",1,"SIMATIC",0.26200000000000001,1,"6AV21030DA050AA5"]
["6AV2103-0DA05-0AH5","SIMATIC WinCC Professional 512 PowerTags V15.1, Engineering software in TIA Portal; Floating License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (64 bit), Windows 10 (64 bit), WinSrv 2012 R2/2016 (64 bit) for configuration of SIMATIC Panels, WinCC Runtime Advanced, WinCC Runtime Professional (512 PowerTags) ******************************* E-mail address required for delivery",2100,"ST",1,"SIMATIC",1E-3,1,"6AV21030DA050AH5"]
["6AV2103-0HA00-0AL0","SIMATIC WinCC Professional 4096 Power Tags, SUS Software Update Service, within the framework of this contract, you will receive for one year all up-to-date software versions, the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software",552,"ST",1,"SIMATIC",1.2E-2,1,"6AV21030HA000AL0"]
["6AV2103-0HA00-0AM0","SIMATIC WinCC Professional 4096 Power Tags, SUS (Compact) Software Update Service, for multiple orders on one position, these deliveries are grouped. Minimum order quantity: 3 units within the framework of this contract, you will receive for one year all up-to-date software versions, the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software",552,"ST",1,"SIMATIC",1.2E-2,1,"6AV21030HA000AM0"]
["6AV2103-0HA00-0AQ0","EPL Royalty for SIMATIC WinCC Professional 4096 Power Tags, only valid in connection with Enterprise License contract, requires EPL Master",2896,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21030HA000AQ0"]
["6AV2103-0HA00-0AR0","EPL Maintenance for SIMATIC WinCC Professional 4096 Power Tags, (EPL=Enterprise License) Payment for maintenance of a Royalty for 12 months, only valid in connection with Enterprise License contract, requires EPL Master",541,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21030HA000AR0"]
["6AV2103-0HA00-0AY0","SIMATIC WinCC Professional 4096 Power Tags, SUS (download) Software Update Service, within the framework of this contract, you will receive for one year all up-to-date software versions, the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software ******************************* E-mail address required for delivery",515,"ST",1,"SIMATIC",1E-3,1,"6AV21030HA000AY0"]
["6AV2103-0HA00-0UA0","SIMATIC WinCC Professional 4096 PowerTags V15.1; UCL package (TIA Portal) for one installation; Engineering software; Software and documentation on DVD; Master license on CD; UCL agreement required",2317,"ST",1,"SIMATIC",0.28699999999999998,1,"6AV21030HA000UA0"]
["6AV2103-0HA00-0UH0","SIMATIC WinCC Professional 4096 PowerTags V15.1, UCL package (TIA Portal) for one installation; Engineering software; Software, documentation and master license for download; UCL agreement required ******************************* E-mail address required for delivery",2100,"ST",1,"SIMATIC",1E-3,1,"6AV21030HA000UH0"]
["6AV2103-0HA00-0UL0","SIMATIC WinCC Professional 4096 Power Tags, SUS (UCL) Software Update Service, Automatic subsequent deliveries of upgrades and service packs for one year with automatic extension, requires current software version, only valid in connection with Unlock Copy License agreement Minimum ordering quantity 20 units",433,"ST",1,"SIMATIC",1.2E-2,1,"6AV21030HA000UL0"]
["6AV2103-0HA00-0UY0","SIMATIC WinCC Professional 4096 Power Tags, SUS (UCL download) Software Update Service, Automatic subsequent deliveries of Upgrades and service packs for one year with automatic extension; requires current software version; only valid in connection with Unlock Copy License agreement; Minimum ordering quantity 20 units ******************************* E-mail address required for delivery",412,"ST",1,"SIMATIC",1E-3,1,"6AV21030HA000UY0"]
["6AV2103-0HA05-0AA5","SIMATIC WinCC Professional 4096 PowerTags V15.1, Engineering software in TIA Portal; Floating License; SW and documentation on DVD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; Windows 7 (64-bit), Windows 10 (64-bit), WinSrv 2012 R2/2016 (64-bit) 2008 R2/2012 R2/2016 (64-bit) for configuration of SIMATIC Panels, WinCC Runtime Advanced, WinCC Runtime Professional (4096 PowerTags) ******************************* Content: Set (3x DVD + 1x USB)",2954,"ST",1,"SIMATIC",0.26200000000000001,1,"6AV21030HA050AA5"]
["6AV2103-0HA05-0AH5","SIMATIC WinCC Professional 4096 PowerTags V15.1, Engineering software in TIA Portal; Floating License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (64 bit), Windows 10 (64 bit), WinSrv 2012 R2/2016 (64 bit) for configuration of SIMATIC Panels, WinCC Runtime Advanced, WinCC Runtime Professional (4096 PowerTags) ******************************* E-mail address required for delivery",2625,"ST",1,"SIMATIC",1E-3,1,"6AV21030HA050AH5"]
["6AV2103-0XA00-0AL0","SIMATIC WinCC Professional max. Power Tags, SUS Software Update Service, within the framework of this contract, you will receive for one year all up-to-date software versions, the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software",884,"ST",1,"SIMATIC",1.2E-2,1,"6AV21030XA000AL0"]
["6AV2103-0XA00-0AM0","SIMATIC WinCC Professional max. Power Tags, SUS (Compact) Software Update Service, for multiple orders on one position, these deliveries are grouped. Minimum order quantity: 3 units within the framework of this contract, you will receive for one year all up-to-date software versions, the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software",884,"ST",1,"SIMATIC",1.2E-2,1,"6AV21030XA000AM0"]
["6AV2103-0XA00-0AQ0","EPL Royalty for SIMATIC WinCC Professional max. Power Tags, only valid in connection with Enterprise License contract, requires EPL Master",4633,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21030XA000AQ0"]
["6AV2103-0XA00-0AQ1","EPL Royalty Service for SIMATIC WinCC Professional max. Power Tags, only valid in connection with Enterprise License contract, requires EPL Master",4633,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21030XA000AQ1"]
["6AV2103-0XA00-0AR0","EPL Maintenance for SIMATIC WinCC Professional max. Power Tags, (EPL=Enterprise License) Payment for maintenance of a Royalty for 12 months, only valid in connection with Enterprise License contract, requires EPL Master",866,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21030XA000AR0"]
["6AV2103-0XA00-0AY0","SIMATIC WinCC Professional max. Power Tags, SUS (download) Software Update Service, within the framework of this contract, you will receive for one year all up-to-date software versions, the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software ******************************* E-mail address required for delivery",824,"ST",1,"SIMATIC",1E-3,1,"6AV21030XA000AY0"]
["6AV2103-0XA00-0UA0","SIMATIC WinCC Professional max. PowerTags V15.1 UCL package (TIA Portal) for one installation; Engineering software; Software and documentation on DVD; Master license on CD; UCL agreement required",3707,"ST",1,"SIMATIC",0.28699999999999998,1,"6AV21030XA000UA0"]
["6AV2103-0XA00-0UH0","SIMATIC WinCC Professional max. PowerTags V15.1 UCL package (TIA Portal) for one installation; Engineering software; Software, documentation and master license for download; UCL agreement required ******************************* E-mail address required for delivery",3360,"ST",1,"SIMATIC",1E-3,1,"6AV21030XA000UH0"]
["6AV2103-0XA00-0UL0","SIMATIC WinCC Professional max. Power Tags, SUS (UCL) Software Update Service, Automatic subsequent deliveries of upgrades and service packs for one year with automatic extension, requires current software version, only valid in connection with Unlock Copy License agreement Minimum ordering quantity 20 units",692,"ST",1,"SIMATIC",1.2E-2,1,"6AV21030XA000UL0"]
["6AV2103-0XA00-0UY0","SIMATIC WinCC Professional max. Power Tags, SUS (UCL download) Software Update Service, Automatic subsequent deliveries of Upgrades and service packs for one year with automatic extension; requires current software version; only valid in connection with Unlock Copy License agreement; Minimum ordering quantity 20 units ******************************* E-mail address required for delivery",659,"ST",1,"SIMATIC",1E-3,1,"6AV21030XA000UY0"]
["6AV2103-0XA05-0AA5","SIMATIC WinCC Professional max. PowerTags V15.1, Engineering software in TIA Portal; Floating License; SW and documentation on DVD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (64-bit), Windows 10 (64-bit), WinSrv 2012 R2/2016 (64-bit) for configuration of SIMATIC Panels, WinCC Runtime Advanced, WinCC Runtime Professional (max. PowerTags) ******************************* Content: Set (3x DVD + 1x USB)",4725,"ST",1,"SIMATIC",0.26200000000000001,1,"6AV21030XA050AA5"]
["6AV2103-0XA05-0AH5","SIMATIC WinCC Professional max. PowerTags V15.1, Engineering software in TIA Portal; Floating License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (64 bit), Windows 10 (64 bit), WinSrv 2012 R2/2016 (64 bit) for configuration of SIMATIC Panels, WinCC Runtime Advanced, WinCC Runtime Professional (max. PowerTags) ******************************* E-mail address required for delivery",4200,"ST",1,"SIMATIC",1E-3,1,"6AV21030XA050AH5"]
["6AV2103-2AD00-0UC0","SIMATIC WinCC Prof. V15.1 UCL (TIA Portal) Powerpack WinCC Advanced V15.1 -> WinCC Professional 512 PowerTags V15.1, for one installation; Engineering software; Software and documentation on DVD; Master license on CD; UCL agreement required",232,"ST",1,"SIMATIC",0.22600000000000001,1,"6AV21032AD000UC0"]
["6AV2103-2AD00-0UJ0","SIMATIC WinCC Professional UCL (TIA Portal) Powerpack WinCC Advanced V15.1 -> WinCC Professional 512 PowerTags V15.1, for one installation; Engineering software; software, documentation and master license for download; UCL agreement required ******************************* E-mail address required for delivery",210,"ST",1,"SIMATIC",1E-3,1,"6AV21032AD000UJ0"]
["6AV2103-2AD05-0BD5","SIMATIC WinCC Professional Powerpack WinCC Advanced -> WinCC Professional 512 PowerTags V15.1 (without version change); engineering software in the TIA Portal; Floating License; Software and documentation on DVD; License key on USB flash drive; Class A ******************************* Content: Set (2x DVD + 1x USB)",297,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21032AD050BD5"]
["6AV2103-2AD05-0BJ5","SIMATIC WinCC Professional Power Pack WinCC Advanced-> WinCC Professional 512 PowerTags V15.1 (without version replacement); Engineering software in TIA Portal; Floating License; Software, documentation and License key for download; Class A ***************************** ** E-mail address required for delivery",263,"ST",1,"SIMATIC",1E-3,1,"6AV21032AD050BJ5"]
["6AV2103-2DH00-0UC0","SIMATIC WinCC Professional V15 UCL (TIA Portal) Power Pack 512 -> 4096 PowerTags V15, for one installation; Engineering software; Master license on CD; UCL agreement required",464,"ST",1,"SIMATIC",0.17599999999999999,1,"6AV21032DH000UC0"]
["6AV2103-2DH00-0UJ0","SIMATIC WinCC Professional UCL (TIA Portal) Power Pack 512 -> 4096 PowerTags V15, for one installation; Engineering software; master license for download; UCL agreement required ******************************* E-mail address required for delivery",420,"ST",1,"SIMATIC",1E-3,1,"6AV21032DH000UJ0"]
["6AV2103-2DH05-0BD5","SIMATIC WinCC Professional Powerpack 512 PowerTags-> 4096 Power Tags V15 (without version change); engineering software in the TIA Portal; Floating License; Without software a. documentation; License key on USB flash drive; Class A ******************************* Content: 1x USB",591,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21032DH050BD5"]
["6AV2103-2DH05-0BJ5","SIMATIC WinCC Professional Powerpack 512 PowerTags -> 4096 PowerTags V15 (no change of version); engineering software in TIA Portal; floating license; license key for download; without software and documentation; class A; ******************************* email address is mandatory for delivery",525,"ST",1,"SIMATIC",1E-3,1,"6AV21032DH050BJ5"]
["6AV2103-2HX00-0UC0","SIMATIC WinCC Professional V15 UCL (TIA Portal) Power Pack 4096 -> max. PowerTags V15, for one installation; Engineering software; Master license on CD; UCL agreement required",1391,"ST",1,"SIMATIC",0.17599999999999999,1,"6AV21032HX000UC0"]
["6AV2103-2HX00-0UJ0","SIMATIC WinCC Professional UCL (TIA Portal) Power Pack 4096 -> max. PowerTags V15, for one installation; Engineering software; master license for download; UCL agreement required ******************************* E-mail address required for delivery",1260,"ST",1,"SIMATIC",1E-3,1,"6AV21032HX000UJ0"]
["6AV2103-2HX05-0BD5","SIMATIC WinCC Professional Powerpack 4096 PowerTags-> max. Power Tags V15 (without version change); engineering software in the TIA Portal; Floating License; Without software a. documentation; License key on USB flash drive; Class A ******************************* Content: 1x USB",1773,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21032HX050BD5"]
["6AV2103-2HX05-0BJ5","SIMATIC WinCC Professional Powerpack 4096 PowerTags -> max. PowerTags V15 (no change of version); engineering software in TIA Portal; floating license; license key for download; without software and documentation; class A; ******************************* email address is mandatory for delivery",1575,"ST",1,"SIMATIC",1E-3,1,"6AV21032HX050BJ5"]
["6AV2103-3DA00-0UE0","SIMATIC WinCC Professional 512 PowerTags V15.1 UCL (TIA Portal) Upgrade V11..V14 -> V15.1; for one installation; Engineering software; Software and documentation on DVD; Master license on CD; UCL agreement required",743,"ST",1,"SIMATIC",0.34200000000000003,1,"6AV21033DA000UE0"]
["6AV2103-3DA00-0UK0","SIMATIC WinCC Professional 512 PowerTags V15.1, UCL (TIA Portal) Upgrade V11..V14 -> V15.1; for one installation; Engineering software; Software, documentation and master license for download; UCL agreement required ******************************* E-mail address required for delivery",672,"ST",1,"SIMATIC",1E-3,1,"6AV21033DA000UK0"]
["6AV2103-3DA05-0AE5","SIMATIC WinCC Professional 512 PowerTags V15.1, Upgrade V11..V14 -> V15.1 or V11..V14 Combo-> V15.1 Combo; engineering software in the TIA Portal; Floating License; SW and documentation on DVD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (64-bit), Windows 10 (64-bit), WinSrv 2012 R2/2016 (64-bit) for configuration of SIMATIC Panels, WinCC Runtime Advanced, WinCC RT Prof. (up to 512 tags) ******************************* Content: Set (5x DVD + 1x USB)",945,"ST",1,"SIMATIC",0.317,1,"6AV21033DA050AE5"]
["6AV2103-3DA05-0AK5","SIMATIC WinCC Professional 512 PowerTags V15.1, Upgrade V11..V14 -> V15.1 or V11..V14 Combo-> V15.1 Combo; Engineering software in TIA Portal; Floating License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (64 bit), Windows 10 (64 bit), WinSrv 2012 R2/2016 (64 bit) for configuring of SIMATIC Panels, WinCC RT Advanced, WinCC RT Prof. (512 PowerTags) ******************************* E-mail address required for delivery",840,"ST",1,"SIMATIC",1E-3,1,"6AV21033DA050AK5"]
["6AV2103-3HA00-0UE0","SIMATIC WinCC Professional 4096 PowerTags V15.1 UCL (TIA Portal) Upgrade V11..V14 -> V15.1; for one installation; Engineering software; Software and documentation on DVD; Master license on CD; UCL agreement required",928,"ST",1,"SIMATIC",0.34200000000000003,1,"6AV21033HA000UE0"]
["6AV2103-3HA00-0UK0","SIMATIC WinCC Professional 4096 PowerTags V15.1, UCL (TIA Portal) Upgrade V11..V14 -> V15.1; for one installation; Engineering software; Software, documentation and master license for download; UCL agreement required ******************************* E-mail address required for delivery",840,"ST",1,"SIMATIC",1E-3,1,"6AV21033HA000UK0"]
["6AV2103-3HA05-0AE5","SIMATIC WinCC Professional 4096 PowerTags V15.1, Upgrade V11..V14 -> V15.1 or V11..V14 Combo-> V15.1 Combo; engineering software in the TIA Portal; Floating License; SW and documentation on DVD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (64-bit), Windows 10 (64-bit), WinSrv 2012 R2/2016 (64-bit) for configuration of SIMATIC Panels, WinCC Runtime Advanced, WinCC RT Prof. (up to 4096 tags) ******************************* Content: Set (5x DVD + 1x USB)",1183,"ST",1,"SIMATIC",0.317,1,"6AV21033HA050AE5"]
["6AV2103-3HA05-0AK5","SIMATIC WinCC Professional 4096 PowerTags V15.1, Upgrade V11..V14 -> V15.1 or V11..V14 Combo-> V15.1 Combo; Engineering software in TIA Portal; Floating License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (64 bit), Windows 10 (64 bit), WinSrv 2012 R2/2016 (64 bit) for configuring of SIMATIC Panels, WinCC RT Advanced, WinCC RT Prof. (4096 PowerTags) ******************************* E-mail address required for delivery",1050,"ST",1,"SIMATIC",1E-3,1,"6AV21033HA050AK5"]
["6AV2103-3XA00-0UE0","SIMATIC WinCC Professional max. PowerTags V15.1 UCL (TIA Portal) Upgrade V11..V14 -> V15.1; for one installation; Engineering software; Software and documentation on DVD; Master license on CD; UCL agreement required",1483,"ST",1,"SIMATIC",0.34200000000000003,1,"6AV21033XA000UE0"]
["6AV2103-3XA00-0UK0","SIMATIC WinCC Professional max. PowerTags V15.1 UCL (TIA Portal) Upgrade V11..V14 -> V15.1; for one installation; Engineering software; Software, documentation and master license for download; UCL agreement required ******************************* E-mail address required for delivery",1344,"ST",1,"SIMATIC",1E-3,1,"6AV21033XA000UK0"]
["6AV2103-3XA05-0AE5","SIMATIC WinCC Professional max. PowerTags V15.1, Upgrade V11..V14 -> V15.1 or V11..V14 Combo-> V15.1 Combo; engineering software in the TIA Portal; Floating License; SW and documentation on DVD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (64-bit), Windows 10 (64-bit), WinSrv 2012 R2/2016 (64-bit) for configuration of SIMATIC Panels, WinCC Runtime Advanced, WinCC RT Prof. (max. tags) ******************************* Content: Set (5x DVD + 1x USB)",1888,"ST",1,"SIMATIC",0.317,1,"6AV21033XA050AE5"]
["6AV2103-3XA05-0AK5","SIMATIC WinCC Professional max. PowerTags V15.1, Upgrade V11..V14 -> V15.1 or V11..V14 Combo-> V15.1 Combo; Engineering software in TIA Portal; Floating License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (64 bit), Windows 10 (64 bit), WinSrv 2012 R2/2016 (64 bit) for configuring of SIMATIC Panels, WinCC RT Advanced, WinCC RT Prof. (max. PowerTags) ******************************* E-mail address required for delivery",1680,"ST",1,"SIMATIC",1E-3,1,"6AV21033XA050AK5"]
["6AV2103-8XA00-0AP0","EPL master for WinCC V15.1 Engineering (EPL=Enterprise License) Mandatory royalty per 1 installation only valid in connection with Enterprise License agreement",314,"ST",1,"SIMATIC",0.27400000000000002,1,"6AV21038XA000AP0"]
["6AV2104-0BA00-0AQ0","EPL Royalty for SIMATIC WinCC Runtime Advanced 128 Power Tags; only valid in connection with Enterprise License contract, requires EPL Master",466,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21040BA000AQ0"]
["6AV2104-0BA00-0AR0","EPL Maintenance for SIMATIC WinCC Runtime Advanced 128 Power Tags; (EPL=Enterprise License) Payment for maintenance of a Royalty for 12 months, only valid in connection with Enterprise License contract, requires EPL Master",89.3,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21040BA000AR0"]
["6AV2104-0BA05-0AA0","SIMATIC WinCC Runtime Advanced 128 PowerTags V15.1, R-SW in TIA Portal; Single License; SW and documentation on DVD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (32-bit, 64-bit), Windows 8.1/10 (64-bit), WinSrv 2008 R2/2012 R2/2016 (64-bit) ******************************* Content: Set (1x DVD + 1x USB)",475,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21040BA050AA0"]
["6AV2104-0BA05-0AH0","SIMATIC WinCC Runtime Advanced 128 PowerTags V15.1, R-SW in TIA Portal; Single License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (32 bit, 64 bit), Windows 8.1/10 (64 bit), WinSrv 2008 R2/2012 R2/2016 (64 bit) ******************************* E-mail address required for delivery",420,"ST",1,"SIMATIC",1E-3,1,"6AV21040BA050AH0"]
["6AV2104-0DA00-0AQ0","EPL Royalty for SIMATIC WinCC Runtime Advanced 512 Power Tags; only valid in connection with Enterprise License contract, requires EPL Master",1505,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21040DA000AQ0"]
["6AV2104-0DA00-0AR0","EPL Maintenance for SIMATIC WinCC Runtime Advanced 512 Power Tags; (EPL=Enterprise License) Payment for maintenance of a Royalty for 12 months, only valid in connection with Enterprise License contract, requires EPL Master",287,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21040DA000AR0"]
["6AV2104-0DA05-0AA0","SIMATIC WinCC Runtime Advanced 512 PowerTags V15.1, R-SW in TIA Portal; Single License; SW and documentation on DVD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (32-bit, 64-bit), Windows 8.1/10 (64-bit), WinSrv 2008 R2/2012 R2/2016 (64-bit) ******************************* Content: Set (1x DVD + 1x USB)",1536,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21040DA050AA0"]
["6AV2104-0DA05-0AH0","SIMATIC WinCC Runtime Advanced 512 PowerTags V15.1, R-SW in TIA Portal; Single License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (32 bit, 64 bit), Windows 8.1/10 (64 bit), WinSrv 2008 R2/2012 R2/2016 (64 bit) ******************************* E-mail address required for delivery",1365,"ST",1,"SIMATIC",1E-3,1,"6AV21040DA050AH0"]
["6AV2104-0FA00-0AQ0","EPL Royalty for SIMATIC WinCC Runtime Advanced 2048 Power Tags; only valid in connection with Enterprise License contract, requires EPL Master",2317,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21040FA000AQ0"]
["6AV2104-0FA00-0AR0","EPL Maintenance for SIMATIC WinCC Runtime Advanced 2048 Power Tags; (EPL=Enterprise License) Payment for maintenance of a Royalty for 12 months, only valid in connection with Enterprise License contract, requires EPL Master",441,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21040FA000AR0"]
["6AV2104-0FA05-0AA0","SIMATIC WinCC Runtime Advanced 2048 PowerTags V15.1, R-SW in TIA Portal; Single License; SW and documentation on DVD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (32-bit, 64-bit), Windows 8.1/10 (64-bit), WinSrv 2008 R2/2012 R2/2016 (64-bit) ******************************* Content: Set (1x DVD + 1x USB)",2363,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21040FA050AA0"]
["6AV2104-0FA05-0AH0","SIMATIC WinCC Runtime Advanced 2048 PowerTags V15.1, R-SW in TIA Portal; Single License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (32 bit, 64 bit), Windows 8.1/10 (64 bit), WinSrv 2008 R2/2012 R2/2016 (64 bit) ******************************* E-mail address required for delivery",2100,"ST",1,"SIMATIC",1E-3,1,"6AV21040FA050AH0"]
["6AV2104-0HA00-0AQ0","EPL Royalty for SIMATIC WinCC Runtime Advanced 4096 Power Tags; only valid in connection with Enterprise License contract, requires EPL Master",3476,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21040HA000AQ0"]
["6AV2104-0HA00-0AR0","EPL Maintenance for SIMATIC WinCC Runtime Advanced 4096 Power Tags; (EPL=Enterprise License) Payment for maintenance of a Royalty for 12 months, only valid in connection with Enterprise License contract, requires EPL Master",662,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21040HA000AR0"]
["6AV2104-0HA05-0AA0","SIMATIC WinCC Runtime Advanced 4096 PowerTags V15.1, R-SW in TIA Portal; Single License; SW and documentation on DVD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (32-bit, 64-bit), Windows 8.1/10 (64-bit), WinSrv 2008 R2/2012 R2/2016 (64-bit) ******************************* Content: Set (1x DVD + 1x USB)",3545,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21040HA050AA0"]
["6AV2104-0HA05-0AH0","SIMATIC WinCC Runtime Advanced 4096 PowerTags V15.1, R-SW in TIA Portal; Single License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (32 bit, 64 bit), Windows 8.1/10 (64 bit), WinSrv 2008 R2/2012 R2/2016 (64 bit) ******************************* E-mail address required for delivery",3150,"ST",1,"SIMATIC",1E-3,1,"6AV21040HA050AH0"]
["6AV2104-0KA00-0AQ0","EPL Royalty for SIMATIC WinCC Runtime Advanced 8192 Power Tags; only valid in connection with Enterprise License contract, requires EPL Master",4633,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21040KA000AQ0"]
["6AV2104-0KA00-0AR0","EPL Maintenance for SIMATIC WinCC Runtime Advanced 8192 Power Tags; (EPL=Enterprise License) Payment for maintenance of a Royalty for 12 months, only valid in connection with Enterprise License contract, requires EPL Master",882,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21040KA000AR0"]
["6AV2104-0KA05-0AA0","SIMATIC WinCC Runtime Advanced 8192 PowerTags V15.1, R-SW in TIA Portal; Single License; SW and documentation on DVD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (32-bit, 64-bit), Windows 8.1/10 (64-bit), WinSrv 2008 R2/2012 R2/2016 (64-bit) ******************************* Content: Set (1x DVD + 1x USB)",4725,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21040KA050AA0"]
["6AV2104-0KA05-0AH0","SIMATIC WinCC Runtime Advanced 8192 PowerTags V15.1, R-SW in TIA Portal; Single License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (32 bit, 64 bit), Windows 8.1/10 (64 bit), WinSrv 2008 R2/2012 R2/2016 (64 bit) ******************************* E-mail address required for delivery",4200,"ST",1,"SIMATIC",1E-3,1,"6AV21040KA050AH0"]
["6AV2104-0LA05-0AA0","SIMATIC WinCC Runtime Advanced 16384 PowerTags V15.1, R-SW in TIA Portal; Single License; SW and documentation on DVD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (32-bit, 64-bit), Windows 8.1/10 (64-bit), WinSrv 2008 R2/2012 R2/2016 (64-bit) ******************************* Content: Set (1x DVD + 1x USB)",6495,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21040LA050AA0"]
["6AV2104-0LA05-0AH0","SIMATIC WinCC Runtime Advanced 16384 PowerTags V15.1, R-SW in TIA Portal; Single License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (32 bit, 64 bit), Windows 8.1/10 (64 bit), WinSrv 2008 R2/2012 R2/2016 (64 bit) ******************************* E-mail address required for delivery",5775,"ST",1,"SIMATIC",1E-3,1,"6AV21040LA050AH0"]
["6AV2104-0XX05-0DG8","SIMATIC WinCC Runtime Advanced V15/V15.1, software without license, use only in connection with valid license for  WinCC Runtime Advanced V15 or V15.1 ******************************* E-mail address required for delivery",31.5,"ST",1,"SIMATIC",1E-3,1,"6AV21040XX050DG8"]
["6AV2104-0XX05-0DU8","SIMATIC WinCC Runtime Advanced V15/V15.1, data carrier without license, use only in connection with valid license for WinCC Runtime Advanced V15 or V15.1 ******************************* Content: Set (2x DVD)",32.200000000000003,"ST",1,"SIMATIC",0.24099999999999999,1,"6AV21040XX050DU8"]
["6AV2104-2BD05-0BD0","SIMATIC WinCC Runtime Advanced Powerpack 128 PowerTags-> 512 PowerTags V15 (without version change); Runtime software in TIA Portal; Single License; Without software a. documentation; License key on USB flash drive; Class A ******************************* Content: 1x USB",1061,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21042BD050BD0"]
["6AV2104-2BD05-0BJ0","SIMATIC WinCC Runtime Advanced PowerPack 128 PowerTags-> 512 PowerTags V15 (without version replacement); Runtime software in TIA Portal; Single License; License key for download; without software a. documentation; Class A; ******************************* e-mail address required for delivery",945,"ST",1,"SIMATIC",1E-3,1,"6AV21042BD050BJ0"]
["6AV2104-2DF05-0BD0","SIMATIC WinCC Runtime Advanced Powerpack 512 PowerTags-> 2048 PowerTags V15 (without version change); Runtime software in TIA Portal; Single License; Without software a. documentation; License key on USB flash drive; Class A ******************************* Content: 1x USB",830,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21042DF050BD0"]
["6AV2104-2DF05-0BJ0","SIMATIC WinCC Runtime Advanced PowerPack 512 PowerTags-> 2048 PowerTags V15 (without version replacement); Runtime software in TIA Portal; Single License; License key for download; without software a. documentation; Class A; ******************************* e-mail address required for delivery",735,"ST",1,"SIMATIC",1E-3,1,"6AV21042DF050BJ0"]
["6AV2104-2FH05-0BD0","SIMATIC WinCC Runtime Advanced Powerpack 2048 PowerTags-> 4096 Power Tags V15 (without version change); Runtime software in TIA Portal; Single License; Without software a. documentation; License key on USB flash drive; Class A ******************************* Content: 1x USB",1183,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21042FH050BD0"]
["6AV2104-2FH05-0BJ0","SIMATIC WinCC Runtime Advanced PowerPack 2048 PowerTags-> 4096 PowerTags V15 (without version replacement); Runtime software in TIA Portal; Single License; License key for download; without software a. documentation; Class A; ******************************* e-mail address required for delivery",1050,"ST",1,"SIMATIC",1E-3,1,"6AV21042FH050BJ0"]
["6AV2104-2HK05-0BD0","SIMATIC WinCC Runtime Advanced Powerpack 4096 PowerTags-> 8192 PowerTags V15 (without version change); Runtime software in TIA Portal; Single License; Without software a. documentation; License key on USB flash drive; Class A ******************************* Content: 1x USB",1183,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21042HK050BD0"]
["6AV2104-2HK05-0BJ0","SIMATIC WinCC Runtime Advanced PowerPack 4096 PowerTags-> 8192 PowerTags V15 (without version replacement); Runtime software in TIA Portal; Single License; License key for download; without software a. documentation; Class A; ******************************* e-mail address required for delivery",1050,"ST",1,"SIMATIC",1E-3,1,"6AV21042HK050BJ0"]
["6AV2104-2KL05-0BD0","SIMATIC WinCC Runtime Advanced Powerpack 8192 PowerTags-> 16384 PowerTags V15 (without version change); Runtime software in TIA Portal; Single License; Without software a. documentation; License key on USB flash drive; Class A ******************************* Content: 1x USB",1772,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21042KL050BD0"]
["6AV2104-2KL05-0BJ0","SIMATIC WinCC Runtime Advanced PowerPack 8192 PowerTags-> 16384 PowerTags V15 (without version replacement); Runtime software in TIA Portal; Single License; License key for download; without software a. documentation; Class A; ******************************* e-mail address required for delivery",1575,"ST",1,"SIMATIC",1E-3,1,"6AV21042KL050BJ0"]
["6AV2104-3BB05-0AE0","SIMATIC WinCC Runtime Advanced 128 PowerTags V15.1, Upgrade V11..V14 -> V15.1; R-SW in TIA Portal; Single License; SW and documentation on DVD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (32-bit, 64-bit), Windows 8.1/10 (64-bit), WinSrv 2008 R2/2012 R2/2016 (64-bit) ******************************* Content: Set (1x DVD + 1x USB)",191,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21043BB050AE0"]
["6AV2104-3BB05-0AK0","SIMATIC WinCC Runtime Advanced 128 PowerTags V15.1, Upgrade V11..V14 -> V15.1; R-SW in TIA Portal; Single License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (32 bit, 64 bit), Windows 8.1/10 (64 bit), WinSrv 2008 R2/2012 R2/2016 (64 bit) ******************************* E-mail address required for delivery",168,"ST",1,"SIMATIC",1E-3,1,"6AV21043BB050AK0"]
["6AV2104-3DD05-0AE0","SIMATIC WinCC Runtime Advanced 512 PowerTags V15.1, Upgrade V11..V14 -> V15.1; R-SW in TIA Portal; Single License; SW and documentation on DVD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (32-bit, 64-bit), Windows 8.1/10 (64-bit), WinSrv 2008 R2/2012 R2/2016 (64-bit) ******************************* Content: Set (1x DVD + 1x USB)",614,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21043DD050AE0"]
["6AV2104-3DD05-0AK0","SIMATIC WinCC Runtime Advanced 512 PowerTags V15.1, Upgrade V11..V14 -> V15.1; R-SW in TIA Portal; Single License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (32 bit, 64 bit), Windows 8.1/10 (64 bit), WinSrv 2008 R2/2012 R2/2016 (64 bit) ******************************* E-mail address required for delivery",546,"ST",1,"SIMATIC",1E-3,1,"6AV21043DD050AK0"]
["6AV2104-3FF05-0AE0","SIMATIC WinCC Runtime Advanced 2048 PowerTags V15.1, Upgrade V11..V14 -> V15.1; R-SW in TIA Portal; Single License; SW and documentation on DVD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (32-bit, 64-bit), Windows 8.1/10 (64-bit), WinSrv 2008 R2/2012 R2/2016 (64-bit) ******************************* Content: Set (1x DVD + 1x USB)",945,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21043FF050AE0"]
["6AV2104-3FF05-0AK0","SIMATIC WinCC Runtime Advanced 2048 PowerTags V15.1, Upgrade V11..V14 -> V15.1; R-SW in TIA Portal; Single License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (32 bit, 64 bit), Windows 8.1/10 (64 bit), WinSrv 2008 R2/2012 R2/2016 (64 bit) ******************************* E-mail address required for delivery",840,"ST",1,"SIMATIC",1E-3,1,"6AV21043FF050AK0"]
["6AV2104-3HH05-0AE0","SIMATIC WinCC Runtime Advanced 4096 PowerTags V15.1, Upgrade V11..V14 -> V15.1; R-SW in TIA Portal; Single License; SW and documentation on DVD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (32-bit, 64-bit), Windows 8.1/10 (64-bit), WinSrv 2008 R2/2012 R2/2016 (64-bit) ******************************* Content: Set (1x DVD + 1x USB)",1420,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21043HH050AE0"]
["6AV2104-3HH05-0AK0","SIMATIC WinCC Runtime Advanced 4096 PowerTags V15.1, Upgrade V11..V14 -> V15.1; R-SW in TIA Portal; Single License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (32 bit, 64 bit), Windows 8.1/10 (64 bit), WinSrv 2008 R2/2012 R2/2016 (64 bit) ******************************* E-mail address required for delivery",1260,"ST",1,"SIMATIC",1E-3,1,"6AV21043HH050AK0"]
["6AV2104-3KK05-0AE0","SIMATIC WinCC Runtime Advanced 8192 or 16384 PowerTags V15.1, Upgrade V11..V14 -> V15.1; R-SW in the TIA Portal; Single License; SW and documentation on DVD; License key on USB flash drive;  Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (32-bit, 64-bit), Windows 8.1/10 (64-bit), WinSrv 2008 R2/2012 R2/2016 (64-bit) ******************************* Content: Set (1x DVD + 1x USB)",1888,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21043KK050AE0"]
["6AV2104-3KK05-0AK0","SIMATIC WinCC Runtime Advanced 8192 or 16384 PowerTags V15.1, Upgrade V11..V14 -> V15.1; R-SW in TIA Portal; Single License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (32 bit, 64 bit), Windows 8.1/10 (64 bit), WinSrv 2008 R2/2012 R2/2016 (64 bit) ******************************* E-mail address required for delivery",1680,"ST",1,"SIMATIC",1E-3,1,"6AV21043KK050AK0"]
["6AV2104-4BB05-0AE0","SIMATIC WinCC Runtime Advanced 128 PowerTags V15.1, Upgrade WinCC flexible 2008 Runtime 128 PowerTags-> WinCC Runtime Advanced 128 PowerTags V15.1; R-SW in TIA Portal; Single License; SW and documentation on DVD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (32-bit, 64-bit), Windows 8.1/10 (64-bit), WinSrv 2008 R2/2012 R2/2016 (64-bit) ******************************* Content: Set (1x DVD + 1x USB)",191,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21044BB050AE0"]
["6AV2104-4BB05-0AK0","SIMATIC WinCC Runtime Advanced 128 PowerTags V15.1, Upgrade WinCC flexible 2008 Runtime 128 PowerTags-> WinCC Runtime Advanced 128 PowerTags V15.1; R-SW in TIA Portal; Single License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (32 bit, 64 bit), Windows 8.1/10 (64 bit), WinSrv 2008 R2/2012 R2/2016 (64 bit) ******************************* E-mail address required for delivery",168,"ST",1,"SIMATIC",1E-3,1,"6AV21044BB050AK0"]
["6AV2104-4DD05-0AE0","SIMATIC WinCC Runtime Advanced 512 PowerTags V15.1, Upgrade WinCC flexible 2008 Runtime 512 PowerTags-> WinCC Runtime Advanced 512 PowerTags V15.1; R-SW in TIA Portal; Single License; SW and documentation on DVD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (32-bit, 64-bit), Windows 8.1/10 (64-bit), WinSrv 2008 R2/2012 R2/2016 (64-bit) ******************************* Content: Set (1x DVD + 1x USB)",614,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21044DD050AE0"]
["6AV2104-4DD05-0AK0","SIMATIC WinCC Runtime Advanced 512 PowerTags V15.1, Upgrade WinCC flexible 2008 Runtime 512 PowerTags-> WinCC Runtime Advanced 512 PowerTags V15.1; R-SW in TIA Portal; Single License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (32 bit, 64 bit), Windows 8.1/10 (64 bit), WinSrv 2008 R2/2012 R2/2016 (64 bit) ******************************* E-mail address required for delivery",546,"ST",1,"SIMATIC",1E-3,1,"6AV21044DD050AK0"]
["6AV2104-4FF05-0AE0","SIMATIC WinCC Runtime Advanced 2048 PowerTags V15.1, Upgrade WinCC flexible 2008 Runtime 2048 PowerTags-> WinCC Runtime Advanced 2048 PowerTags V15.1; R-SW in TIA Portal; Single License; SW and documentation on DVD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (32-bit, 64-bit), Windows 8.1/10 (64-bit), WinSrv 2008 R2/2012 R2/2016 (64-bit) ******************************* Content: Set (1x DVD + 1x USB)",945,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21044FF050AE0"]
["6AV2104-4FF05-0AK0","SIMATIC WinCC Runtime Advanced 2048 PowerTags V15.1, Upgrade WinCC flexible 2008 Runtime 2048 PowerTags-> WinCC Runtime Advanced 2048 PowerTags V15.1; R-SW in TIA Portal; Single License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (32 bit, 64 bit), Windows 8.1/10 (64 bit), WinSrv 2008 R2/2012 R2/2016 (64 bit) ******************************* E-mail address required for delivery",840,"ST",1,"SIMATIC",1E-3,1,"6AV21044FF050AK0"]
["6AV2104-4HH05-0AE0","SIMATIC WinCC Runtime Advanced 4096 PowerTags V15.1, Upgrade WinCC flexible 2008 Runtime 4096 PowerTags-> WinCC Runtime Advanced 4096 PowerTags V15.1; R-SW in TIA Portal; Single License; SW and documentation on DVD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (32-bit, 64-bit), Windows 8.1/10 (64-bit), WinSrv 2008 R2/2012 R2/2016 (64-bit) ******************************* Content: Set (1x DVD + 1x USB)",1420,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21044HH050AE0"]
["6AV2104-4HH05-0AK0","SIMATIC WinCC Runtime Advanced 4096 PowerTags V15.1, Upgrade WinCC flexible 2008 Runtime 4096 PowerTags-> WinCC Runtime Advanced 4096 PowerTags V15.1; R-SW in TIA Portal; Single License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (32 bit, 64 bit), Windows 8.1/10 (64 bit), WinSrv 2008 R2/2012 R2/2016 (64 bit) ******************************* E-mail address required for delivery",1260,"ST",1,"SIMATIC",1E-3,1,"6AV21044HH050AK0"]
["6AV2104-4KK05-0AE0","SIMATIC WinCC Runtime Advanced 8192 PowerTags V15.1, Upgrade WinCC flexible 2008 Runtime 8000 PowerTags-> WinCC Runtime Advanced 8192 PowerTags V15.1; R-SW in TIA Portal; Single License; SW and documentation on DVD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; Executable in Windows 7 (32-bit, 64-bit), Windows 8.1/10 (64-bit), WinSrv 2008 R2/2012 R2/2016 (64-bit) ******************************* Content: Set (1x DVD + 1x USB)",1888,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21044KK050AE0"]
["6AV2104-4KK05-0AK0","SIMATIC WinCC Runtime Advanced 8192 PowerTags V15.1, Upgrade WinCC flexible 2008 Runtime 8000 PowerTags-> WinCC Runtime Advanced 8192 PowerTags V15.1; R-SW in TIA Portal; Single License; Software, documentation and License key for download; Class A; 6 languages: de, en, fr, es, it, zh; executable under Windows 7 (32 bit, 64 bit), Windows 8.1/10 (64 bit), WinSrv 2008 R2/2012 R2/2016 (64 bit) ******************************* E-mail address required for delivery",1680,"ST",1,"SIMATIC",1E-3,1,"6AV21044KK050AK0"]
["6AV2104-8XA00-0AP0","EPL Master for WinCC Runtime Advanced V15.1 (EPL=Enterprise License); Mandatory royalty per 1 installation; only valid in connection with Enterprise License agreement",314,"ST",1,"SIMATIC",0.224,1,"6AV21048XA000AP0"]
["6AV2105-0BA05-0AA0","SIMATIC WinCC RT Professional, 128 PowerTags V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit)/ ******************************* Content: Set (2x DVD + 1x USB)",2667,"ST",1,"SIMATIC",0.252,1,"6AV21050BA050AA0"]
["6AV2105-0BA05-0AH0","SIMATIC WinCC RT Professional, 128 PowerTags V15.1, Runtime software in TIA Portal, Single license, software and documentation download, License key download, Class A, 5 languages (de, en, fr, es, it) executable under Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit) ******************************* E-mail address required for delivery",2371,"ST",1,"SIMATIC",1E-3,1,"6AV21050BA050AH0"]
["6AV2105-0BA15-0AA0","SIMATIC WinCC RT Professional, 128 PowerTags Asia V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 6 languages (de,en,fr,es,it,zh), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",2667,"ST",1,"SIMATIC",0.253,1,"6AV21050BA150AA0"]
["6AV2105-0DA05-0AA0","SIMATIC WinCC RT Professional, 512 PowerTags V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit)/ ******************************* Content: Set (2x DVD + 1x USB)",4123,"ST",1,"SIMATIC",0.252,1,"6AV21050DA050AA0"]
["6AV2105-0DA05-0AH0","SIMATIC WinCC RT Professional, 512 PowerTags V15.1, Runtime software in TIA Portal, Single license, software and documentation download, License key download, Class A, 5 languages (de, en, fr, es, it) executable under Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit) ******************************* E-mail address required for delivery",3666,"ST",1,"SIMATIC",1E-3,1,"6AV21050DA050AH0"]
["6AV2105-0DA15-0AA0","SIMATIC WinCC RT Professional, 512 PowerTags Asia V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 6 languages (de,en,fr,es,it,zh), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",4123,"ST",1,"SIMATIC",0.253,1,"6AV21050DA150AA0"]
["6AV2105-0FA05-0AA0","SIMATIC WinCC RT Professional, 2048 PowerTags V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit)/ ******************************* Content: Set (2x DVD + 1x USB)",5054,"ST",1,"SIMATIC",0.252,1,"6AV21050FA050AA0"]
["6AV2105-0FA05-0AH0","SIMATIC WinCC RT Professional, 2048 PowerTags V15.1, Runtime software in TIA Portal, Single license, software and documentation download, License key download, Class A, 5 languages (de, en, fr, es, it) executable under Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit) ******************************* E-mail address required for delivery",4494,"ST",1,"SIMATIC",1E-3,1,"6AV21050FA050AH0"]
["6AV2105-0FA15-0AA0","SIMATIC WinCC RT Professional, 2048 PowerTags Asia V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 6 languages (de,en,fr,es,it,zh), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",5054,"ST",1,"SIMATIC",0.253,1,"6AV21050FA150AA0"]
["6AV2105-0HA05-0AA0","SIMATIC WinCC RT Professional, 4096 PowerTags V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit)/ ******************************* Content: Set (2x DVD + 1x USB)",5579,"ST",1,"SIMATIC",0.252,1,"6AV21050HA050AA0"]
["6AV2105-0HA05-0AH0","SIMATIC WinCC RT Professional, 4096 PowerTags V15.1, Runtime software in TIA Portal, Single license, software and documentation download, License key download, Class A, 5 languages (de, en, fr, es, it) executable under Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit) ******************************* E-mail address required for delivery",4962,"ST",1,"SIMATIC",1E-3,1,"6AV21050HA050AH0"]
["6AV2105-0HA05-0AS0","SCE Trainer Package HMI WinCC WinCC Professional max. V15 WinCC RT Professional 4096 V15 contains: SW and documentation on DVD, 6 user-lic. on USB stick, for WinCC Professional V15Engineering, Runtime, Optionen for educational purposes only",2689,"ST",1,"SIMATIC",0.36099999999999999,1,"6AV21050HA050AS0"]
["6AV2105-0HA15-0AA0","SIMATIC WinCC RT Professional, 4096 PowerTags Asia V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 6 languages (de,en,fr,es,it,zh), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",5579,"ST",1,"SIMATIC",0.253,1,"6AV21050HA150AA0"]
["6AV2105-0KA05-0AA0","SIMATIC WinCC RT Professional, 8192 PowerTags V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit)/ ******************************* Content: Set (2x DVD + 1x USB)",6075,"ST",1,"SIMATIC",0.252,1,"6AV21050KA050AA0"]
["6AV2105-0KA05-0AH0","SIMATIC WinCC RT Professional, 8192 PowerTags V15.1, Runtime software in TIA Portal, Single license, software and documentation download, License key download, Class A, 5 languages (de, en, fr, es, it) executable under Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit) ******************************* E-mail address required for delivery",5403,"ST",1,"SIMATIC",1E-3,1,"6AV21050KA050AH0"]
["6AV2105-0KA15-0AA0","SIMATIC WinCC RT Professional, 8192 PowerTags Asia V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 6 languages (de,en,fr,es,it,zh), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",6075,"ST",1,"SIMATIC",0.253,1,"6AV21050KA150AA0"]
["6AV2105-0MA05-0AA0","SIMATIC WinCC RT Professional, 65536 PowerTags V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit)/ ******************************* Content: Set (2x DVD + 1x USB)",7469,"ST",1,"SIMATIC",0.252,1,"6AV21050MA050AA0"]
["6AV2105-0MA05-0AH0","SIMATIC WinCC RT Professional, 65536 PowerTags V15.1, Runtime software in TIA Portal, Single license, software and documentation download, License key download, Class A, 5 languages (de, en, fr, es, it) executable under Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit) ******************************* E-mail address required for delivery",6643,"ST",1,"SIMATIC",1E-3,1,"6AV21050MA050AH0"]
["6AV2105-0MA15-0AA0","SIMATIC WinCC RT Professional, 65536 PowerTags Asia V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 6 languages (de,en,fr,es,it,zh), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",7469,"ST",1,"SIMATIC",0.253,1,"6AV21050MA150AA0"]
["6AV2105-0PA05-0AA0","SIMATIC WinCC RT Professional, 102400 PowerTags V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit)/ ******************************* Content: Set (2x DVD + 1x USB)",10478,"ST",1,"SIMATIC",0.252,1,"6AV21050PA050AA0"]
["6AV2105-0PA05-0AH0","SIMATIC WinCC RT Professional, 102400 PowerTags V15.1, Runtime software in TIA Portal, Single license, software and documentation download, License key download, Class A, 5 languages (de, en, fr, es, it) executable under Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit) ******************************* E-mail address required for delivery",9317,"ST",1,"SIMATIC",1E-3,1,"6AV21050PA050AH0"]
["6AV2105-0PA15-0AA0","SIMATIC WinCC RT Professional, 102400 PowerTags Asia V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 6 languages (de,en,fr,es,it,zh), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",10478,"ST",1,"SIMATIC",0.253,1,"6AV21050PA150AA0"]
["6AV2105-0RA00-0AP0","SIMATIC WinCC RT Prof V15.1 EPL master (EPL=Enterprise License) Mandatory royalty per 1 installation Only valid in connection with Enterprise License contract",1250,"ST",1,"SIMATIC",0.27400000000000002,1,"6AV21050RA000AP0"]
["6AV2105-0RA00-0AQ0","EPL royalty for SIMATIC WinCC Runtime Professional, for Version V15 for contract No. 00011-GB8 max. Power Tags, (EPL=Enterprise License) only valid in connection with Enterprise License contract, requires EPL Master",2090,"ST",1,"SIMATIC",1.2E-2,1,"6AV21050RA000AQ0"]
["6AV2105-0RA00-0AR0","EPL Maintenance for SIMATIC WinCC Runtime Professional, for contract No. 00011-GB8 max. Power Tags, (EPL=Enterprise License) Payment for maintenance of a royalty for 12 months, only valid in connection with Enterprise License contract, requires EPL Master",2426,"ST",1,"SIMATIC",1.2E-2,1,"6AV21050RA000AR0"]
["6AV2105-0RA05-0AA0","SIMATIC WinCC RT Professional, 153600 PowerTags V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit)/ ******************************* Content: Set (2x DVD + 1x USB)",13639,"ST",1,"SIMATIC",0.252,1,"6AV21050RA050AA0"]
["6AV2105-0RA05-0AH0","SIMATIC WinCC RT Professional, 153600 PowerTags V15.1, Runtime software in TIA Portal, Single license, software and documentation download, License key download, Class A, 5 languages (de, en, fr, es, it) executable under Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit) ******************************* E-mail address required for delivery",12128,"ST",1,"SIMATIC",1E-3,1,"6AV21050RA050AH0"]
["6AV2105-0RA15-0AA0","SIMATIC WinCC RT Professional, 153600 PowerTags Asia V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 6 languages (de,en,fr,es,it,zh), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",13639,"ST",1,"SIMATIC",0.253,1,"6AV21050RA150AA0"]
["6AV2105-0TA05-0AA0","SIMATIC WinCC RT Professional, 262144 PowerTags V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit)/ ******************************* Content: Set (2x DVD + 1x USB)",18722,"ST",1,"SIMATIC",0.252,1,"6AV21050TA050AA0"]
["6AV2105-0TA05-0AH0","SIMATIC WinCC RT Professional, 262144 PowerTags V15.1, Runtime software in TIA Portal, Single license, software and documentation download, License key download, Class A, 5 languages (de, en, fr, es, it) executable under Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit) ******************************* E-mail address required for delivery",16648,"ST",1,"SIMATIC",1E-3,1,"6AV21050TA050AH0"]
["6AV2105-0TA15-0AA0","SIMATIC WinCC RT Professional, 262144 PowerTags Asia V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 6 languages (de,en,fr,es,it,zh), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",18722,"ST",1,"SIMATIC",0.253,1,"6AV21050TA150AA0"]
["6AV2105-0VA05-0AA0","SIMATIC WinCC RT Professional, 500000 Power Tags V15, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), executable in Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit)/ ******************************* Only available for plant engineering (BMW project)",12836,"ST",1,"SIMATIC",0.252,1,"6AV21050VA050AA0"]
["6AV2105-0VA05-0AH0","SIMATIC WinCC RT Professional, 500000 Power Tags V15, runtime software in TIA Portal, single license, software and documentation download, License key download, Class A, 5 languages (de,en,fr,es,it), executable in Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit) ******************************* E-mail address required for delivery ******************************* Only available for plant engineering (BMW project)",3861,"ST",1,"SIMATIC",1E-3,1,"6AV21050VA050AH0"]
["6AV2105-0VA05-0AH1","SIMATIC WinCC RT Professional, 500000 PowerTags V15.1, runtime software in TIA Portal, single license, software and documentation download, license key download, Class A, 5 languages (de,en,fr,es,it), executable in Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64 bit) ******************************* E-mail address required for delivery",30799,"ST",1,"SIMATIC",1E-3,1,"6AV21050VA050AH1"]
["6AV2105-0VA15-0AA0","SIMATIC WinCC RT Professional, 500000 Power Tags Asia V15, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 6 languages (de,en,fr,es,it,zh), executable in Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit)/ ******************************* Only available for plant engineering (BMW project)",12836,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV21050VA150AA0"]
["6AV2105-0XA00-0AL0","SIMATIC WinCC RT Professional Software Update Service (SUS); Within the framework of this contract, you will receive updated software versions for a period of one year, if it is not cancelled three months prior to its expiration. Period of delivery and performance: 1 year from date of invoice. Prerequisite for contract: Current version of the software",1294,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21050XA000AL0"]
["6AV2105-0XA00-0AY0","SIMATIC WinCC RT Professional Software Update Service (SUS); Software Update Service, Within the framework of this contract, you will receive updated software versions for a period of one year, if it is not cancelled three months prior to its expiration. Period of delivery and performance: 1 year from date of invoice. Prerequisite for contract: Current version of the software ******************************* email address is mandatory for delivery",1208,"ST",1,"SIMATIC",1E-3,1,"6AV21050XA000AY0"]
["6AV2105-0XX02-0DU8","WinCC Runtime Professional Update V12-> V12 SP1, data carrier without license, use only in connection with valid license for WinCC Runtime Professional, 6 languages (de,en,fr,es,it,zh), executable in Windows XP (32 bit)/ Windows 7 (32/64 bit) Windows Server 2003 R2/2008 (32 bit)/ Windows Server 2008 R2 (64 bit)",30.5,"ST",1,"SIMATIC",0.191,1,"6AV21050XX020DU8"]
["6AV2105-0XX03-2DU8","WinCC Runtime Professional Data carrier V13 SP2, data carrier without license, use only in connection with valid license for WinCC Runtime Professional, Class A, 6 languages (de,en,fr,es,it,zh), executable in Windows 7 Prof/Ent/Ult +SP1 (32 bit)/ 7 Prof/Ent/Ult +SP1 (64 bit)/ 8.1 Std/Prof/Ent/Ult (64 bit)/ 10 Std/Prof/Ent (64 bit)/ Server 2016 (64 bit) Server 2012 (64 bit) Server 2008 R2+SP1 (64 bit)/",254,"ST",1,"SIMATIC",0.24199999999999999,1,"6AV21050XX032DU8"]
["6AV2105-0XX04-0DU8","WinCC Runtime Professional Update V14-> V14 SP1, data carrier without license, use only in connection with valid license for WinCC Runtime Professional, Class A, 6 languages (de,en,fr,es,it,zh), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Std/Prof/Ent/Ult (64-bit)/ 10 Std/Prof/Ent/Ult (64-bit)/ Server 2016 (64-bit) Server 2012 (64-bit) Server 2008 R2+SP1 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",31.1,"ST",1,"SIMATIC",0.24099999999999999,1,"6AV21050XX040DU8"]
["6AV2105-0XX05-0DG8","SIMATIC WinCC RT Professional V15/V15.1, software without license, use only in connection with valid license for WinCC Runtime Professional V15 or V15.1 ******************************* E-mail address required for delivery",31.5,"ST",1,"SIMATIC",1E-3,1,"6AV21050XX050DG8"]
["6AV2105-0XX05-0DU8","SIMATIC WinCC RT Professional V15/V15.1, data carrier without license, use only in connection with valid license for WinCC Runtime Professional V15 or V15.1 ******************************* Content: Set (2x DVD)",32.200000000000003,"ST",1,"SIMATIC",0.34100000000000003,1,"6AV21050XX050DU8"]
["6AV2105-1VA04-0AH0","SIMATIC WinCC RT Professional, 500000 Power Tags V14 SP1, runtime software in TIA Portal, single license, SW and license key download, Class A, 6 languages (de,en,fr,es,it,zh), executable in Windows 7 Prof/Ent/Ult SP1 (32/64 bit)/ 10 Prof/Ent (64 bit)/ 8.1 Std/Prof/Ent/Ult (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit) ******************************* E-mail address required for delivery ******************************* Only available for for BMW projects",17220,"ST",1,"SIMATIC",1E-3,1,"6AV21051VA040AH0"]
["6AV2105-2BD05-0BD0","SIMATIC WinCC RT Professional, Powerpack 128 PowerTags -> 512 PowerTags V15 / Asia V15 (without version change), runtime software in TIA Portal, single license, without SW, without documentation, License key on USB flash drive, Class A, ******************************* Content: 1x USB",1458,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21052BD050BD0"]
["6AV2105-2BD05-0BJ0","SIMATIC WinCC RT Professional, PowerPack 128 PowerTags -> 512 PowerTags V15 (without version change), runtime software in TIA Portal, Single license, without SW, without documentation, License key download, Class A, ******************************* E-mail address required for delivery",1296,"ST",1,"SIMATIC",1E-3,1,"6AV21052BD050BJ0"]
["6AV2105-2DF05-0BD0","SIMATIC WinCC RT Professional, Powerpack 512 PowerTags -> 2048 PowerTags V15 / Asia V15 (without version change), runtime software in TIA Portal, single license, without SW, without documentation, License key on USB flash drive, Class A, ******************************* Content: 1x USB",931,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21052DF050BD0"]
["6AV2105-2DF05-0BJ0","SIMATIC WinCC RT Professional, PowerPack 512 PowerTags -> 2048 PowerTags V15 (without version change), runtime software in TIA Portal, Single license, without SW, without documentation, License key download, Class A, ******************************* E-mail address required for delivery",828,"ST",1,"SIMATIC",1E-3,1,"6AV21052DF050BJ0"]
["6AV2105-2FH05-0BD0","SIMATIC WinCC RT Professional, Powerpack 2048 PowerTags -> 4096 PowerTags V15 / Asia V15 (without version change), runtime software in TIA Portal, single license, without SW, without documentation, License key on USB flash drive, Class A, ******************************* Content: 1x USB",527,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21052FH050BD0"]
["6AV2105-2FH05-0BJ0","SIMATIC WinCC RT Professional, PowerPack 2048 PowerTags -> 4096 PowerTags V15 (without version change), runtime software in TIA Portal, Single license, without SW, without documentation, License key download, Class A, ******************************* E-mail address required for delivery",469,"ST",1,"SIMATIC",1E-3,1,"6AV21052FH050BJ0"]
["6AV2105-2HK05-0BD0","SIMATIC WinCC RT Professional, Powerpack 4096 PowerTags -> 8192 PowerTags V15 / Asia V15 (without version change), runtime software in TIA Portal, single license, without SW, without documentation, License key on USB flash drive, Class A, ******************************* Content: 1x USB",496,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21052HK050BD0"]
["6AV2105-2HK05-0BJ0","SIMATIC WinCC RT Professional, PowerPack 4096 PowerTags -> 8192 PowerTags V15 (without version change), runtime software in TIA Portal, Single license, without SW, without documentation, License key download, Class A, ******************************* E-mail address required for delivery",441,"ST",1,"SIMATIC",1E-3,1,"6AV21052HK050BJ0"]
["6AV2105-2KM05-0BD0","SIMATIC WinCC RT Professional, Powerpack 8192 PowerTags -> 65535 PowerTags V15 / Asia V15 (without version change), runtime software in TIA Portal, single license, without SW, without documentation, License key on USB flash drive, Class A, ******************************* Content: 1x USB",1395,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21052KM050BD0"]
["6AV2105-2KM05-0BJ0","SIMATIC WinCC RT Professional, PowerPack 8192 PowerTags -> 65535 PowerTags V15 (without version change), runtime software in TIA Portal, Single license, without SW, without documentation, License key download, Class A, ******************************* E-mail address required for delivery",1241,"ST",1,"SIMATIC",1E-3,1,"6AV21052KM050BJ0"]
["6AV2105-2MP05-0BD0","SIMATIC WinCC RT Professional, Powerpack 65535 PowerTags -> 102400 PowerTags V15 / Asia V15 (without version change), runtime software in TIA Portal, single license, without SW, without documentation, License key on USB flash drive, Class A, ******************************* Content: 1x USB",3007,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21052MP050BD0"]
["6AV2105-2MP05-0BJ0","SIMATIC WinCC RT Professional, PowerPack 65535 PowerTags -> 102400 PowerTags V15 (without version change), runtime software in TIA Portal, Single license, without SW, without documentation, License key download, Class A, ******************************* E-mail address required for delivery",2674,"ST",1,"SIMATIC",1E-3,1,"6AV21052MP050BJ0"]
["6AV2105-2PR05-0BD0","SIMATIC WinCC RT Professional, Powerpack 102400 PowerTags -> 153600 PowerTags V15 / Asia V15 (without version change), runtime software in TIA Portal, single license, without SW, without documentation, License key on USB flash drive, Class A, ******************************* Content: 1x USB",3163,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21052PR050BD0"]
["6AV2105-2PR05-0BJ0","SIMATIC WinCC RT Professional, PowerPack 102400 PowerTags -> 153600 PowerTags V15 (without version change), runtime software in TIA Portal, Single license, without SW, without documentation, License key download, Class A, ******************************* E-mail address required for delivery",2812,"ST",1,"SIMATIC",1E-3,1,"6AV21052PR050BJ0"]
["6AV2105-2RT05-0BD0","SIMATIC WinCC RT Professional, Powerpack 153600 PowerTags -> 262144 PowerTags V15 / Asia V15 (without version change), runtime software in TIA Portal, single license, without SW, without documentation, License key on USB flash drive, Class A, ******************************* Content: 1x USB",5084,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21052RT050BD0"]
["6AV2105-2RT05-0BJ0","SIMATIC WinCC RT Professional, PowerPack 153600 PowerTags -> 262144 PowerTags V15 (without version change), runtime software in TIA Portal, Single license, without SW, without documentation, License key download, Class A, ******************************* E-mail address required for delivery",4521,"ST",1,"SIMATIC",1E-3,1,"6AV21052RT050BJ0"]
["6AV2105-3BB05-0AE0","SIMATIC WinCC RT Professional, 128 PowerTags V15.1, Upgrade V11..V14 -> V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit)/ ******************************* Content: Set (2x DVD + 1x USB)",1066,"ST",1,"SIMATIC",0.252,1,"6AV21053BB050AE0"]
["6AV2105-3BB05-0AK0","SIMATIC WinCC RT Professional, 128 PowerTags V15.1, Upgrade V11..V14 -> V15.1, Runtime software in TIA Portal, Single license, software and documentation download, License key download, Class A, 5 languages (de, en, fr, es, it) executable under Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit) ******************************* E-mail address required for delivery",949,"ST",1,"SIMATIC",1E-3,1,"6AV21053BB050AK0"]
["6AV2105-3DD05-0AE0","SIMATIC WinCC RT Professional, 512 PowerTags V15.1, Upgrade V11..V14 -> V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit)/ ******************************* Content: Set (2x DVD + 1x USB)",1650,"ST",1,"SIMATIC",0.252,1,"6AV21053DD050AE0"]
["6AV2105-3DD05-0AK0","SIMATIC WinCC RT Professional, 512 PowerTags V15.1, Upgrade V11..V14 -> V15.1, Runtime software in TIA Portal, Single license, software and documentation download, License key download, Class A, 5 languages (de, en, fr, es, it) executable under Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit) ******************************* E-mail address required for delivery",1467,"ST",1,"SIMATIC",1E-3,1,"6AV21053DD050AK0"]
["6AV2105-3FF05-0AE0","SIMATIC WinCC RT Professional, 2048 PowerTags V15.1, Upgrade V11..V14 -> V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit)/ ******************************* Content: Set (2x DVD + 1x USB)",2023,"ST",1,"SIMATIC",0.252,1,"6AV21053FF050AE0"]
["6AV2105-3FF05-0AK0","SIMATIC WinCC RT Professional, 2048 PowerTags V15.1, Upgrade V11..V14 -> V15.1, Runtime software in TIA Portal, Single license, software and documentation download, License key download, Class A, 5 languages (de, en, fr, es, it) executable under Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit) ******************************* E-mail address required for delivery",1798,"ST",1,"SIMATIC",1E-3,1,"6AV21053FF050AK0"]
["6AV2105-3HH05-0AE0","SIMATIC WinCC RT Professional, 4096 PowerTags V15.1, Upgrade V11..V14 -> V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit)/ ******************************* Content: Set (2x DVD + 1x USB)",2233,"ST",1,"SIMATIC",0.252,1,"6AV21053HH050AE0"]
["6AV2105-3HH05-0AK0","SIMATIC WinCC RT Professional, 4096 PowerTags V15.1, Upgrade V11..V14 -> V15.1, Runtime software in TIA Portal, Single license, software and documentation download, License key download, Class A, 5 languages (de, en, fr, es, it) executable under Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit) ******************************* E-mail address required for delivery",1985,"ST",1,"SIMATIC",1E-3,1,"6AV21053HH050AK0"]
["6AV2105-3KK05-0AE0","SIMATIC WinCC RT Professional, 8192 PowerTags V15.1, Upgrade V11..V14 -> V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit)/ ******************************* Content: Set (2x DVD + 1x USB)",2430,"ST",1,"SIMATIC",0.252,1,"6AV21053KK050AE0"]
["6AV2105-3KK05-0AK0","SIMATIC WinCC RT Professional, 8192 PowerTags V15.1, Upgrade V11..V14 -> V15.1, Runtime software in TIA Portal, Single license, software and documentation download, License key download, Class A, 5 languages (de, en, fr, es, it) executable under Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit) ******************************* E-mail address required for delivery",2161,"ST",1,"SIMATIC",1E-3,1,"6AV21053KK050AK0"]
["6AV2105-3MM05-0AE0","SIMATIC WinCC RT Professional, 64k-256k PowerTags V15.1, Upgrade V11..V14 -> V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit)/ ******************************* Content: Set (2x DVD + 1x USB)",2989,"ST",1,"SIMATIC",0.252,1,"6AV21053MM050AE0"]
["6AV2105-3MM05-0AK0","SIMATIC WinCC RT Professional, 64k-256k PowerTags V15.1, Upgrade V11..V14 -> V15.1, Runtime software in TIA Portal, Single license, software and documentation download, License key download, Class A, 5 languages (de, en, fr, es, it) executable under Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit) ******************************* E-mail address required for delivery",2657,"ST",1,"SIMATIC",1E-3,1,"6AV21053MM050AK0"]
["6AV2105-4BB05-0AE0","SIMATIC WinCC RT Prof V15.1, upgrade WinCC V7.0..V7.4 RT/RC 128 PowerTags -> WinCC Runtime Professional 128 PowerTags V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit)/ ******************************* Content: Set (2x DVD + 1x USB)",1066,"ST",1,"SIMATIC",0.252,1,"6AV21054BB050AE0"]
["6AV2105-4BB05-0AK0","SIMATIC WinCC RT Prof V15.1, upgrade WinCC V7.0..V7.4 RT/RC 128 PowerTags -> WinCC Runtime Professional 128 PowerTags V15.1, Runtime software in the TIA Portal, Single license, software and license key download, Class A, 5 languages (de,en,fr,es,it), Runs under Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit) ******************************* E-mail address is required for delivery",949,"ST",1,"SIMATIC",1E-3,1,"6AV21054BB050AK0"]
["6AV2105-4DD05-0AE0","SIMATIC WinCC RT Prof V15.1, upgrade WinCC V7.0..V7.4 RT/RC 512 PowerTags -> WinCC Runtime Professional 512 PowerTags V15.1, runtime software in the TIA Portal, single license, SW and documentation on DVD, license key on USB stick, Class A, 5 languages (de,en,fr,es,it), executable under Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit)/ ******************************* Content: block (2x DVD + 1x USB)",1650,"ST",1,"SIMATIC",0.252,1,"6AV21054DD050AE0"]
["6AV2105-4DD05-0AK0","SIMATIC WinCC RT Prof V15.1, upgrade WinCC V7.0..V7.4 RT/RC 512 PowerTags -> WinCC Runtime Professional 512 PowerTags V15.1, runtime software in TIA Portal, single license, SW and license key download, Class A, 5 languages (de,en,fr,es,it), executable in Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit) ******************************* E-mail address required for delivery",1467,"ST",1,"SIMATIC",1E-3,1,"6AV21054DD050AK0"]
["6AV2105-4FF05-0AE0","SIMATIC WinCC RT Prof V15.1, upgrade WinCC V7.0..V7.4 RT/RC 2048 PowerTags -> WinCC Runtime Professional 2048 PowerTags V15.1, runtime software in the TIA Portal, single license, SW and documentation on DVD, license key on USB stick, Class A, 5 languages (de,en,fr,es,it), executable under Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit)/ ******************************* Content: block (2x DVD + 1x USB)",2023,"ST",1,"SIMATIC",0.252,1,"6AV21054FF050AE0"]
["6AV2105-4FF05-0AK0","SIMATIC WinCC RT Prof V15.1, upgrade WinCC V7.0..V7.4 RT/RC 2048 PowerTags -> WinCC Runtime Professional 2048 PowerTags V15.1, runtime software in TIA Portal, single license, SW and license key download, Class A, 5 languages (de,en,fr,es,it), executable in Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit) ******************************* E-mail address required for delivery",1798,"ST",1,"SIMATIC",1E-3,1,"6AV21054FF050AK0"]
["6AV2105-4HA05-0AS0","SCE Trainer Package HMI Upgrade WinCC Professional max. V15/ WinCC RT Professional 4096 V15 contains: SW and documentation on DVD, 6 user-lic. on USB stick, for WinCC Professional V15 Engineering, Runtime, Optionen for educational purposes only",975,"ST",1,"SIMATIC",0.40600000000000003,1,"6AV21054HA050AS0"]
["6AV2105-4KK05-0AE0","SIMATIC WinCC RT Prof V15.1, upgrade WinCC V7.0..V7.4 RT/RC 8192 PowerTags -> WinCC Runtime Professional 8192 PowerTags V15.1, runtime software in the TIA Portal, single license, SW and documentation on DVD, license key on USB stick, Class A, 5 languages (de,en,fr,es,it), executable under Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit)/ ******************************* Content: block (2x DVD + 1x USB)",2430,"ST",1,"SIMATIC",0.252,1,"6AV21054KK050AE0"]
["6AV2105-4KK05-0AK0","SIMATIC WinCC RT Prof V15.1, upgrade WinCC V7.0..V7.4 RT/RC 8192 PowerTags -> WinCC Runtime Professional 8192 PowerTags V15.1, runtime software in TIA Portal, single license, SW and license key download, Class A, 5 languages (de,en,fr,es,it), executable in Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit) ******************************* E-mail address required for delivery",2161,"ST",1,"SIMATIC",1E-3,1,"6AV21054KK050AK0"]
["6AV2105-4MM05-0AE0","SIMATIC WinCC RT Prof V15.1, upgrade WinCC V7.0..V7.4 RT/RC 64k-256k PowerTags -> WinCC Runtime Professional 64k-256k PowerTags V15.1, runtime software in the TIA Portal, single license, SW and documentation on DVD, license key on USB stick, Class A, 5 languages (de,en,fr,es,it), executable under Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit)/ ******************************* Content: block (2x DVD + 1x USB)",2989,"ST",1,"SIMATIC",0.252,1,"6AV21054MM050AE0"]
["6AV2105-4MM05-0AK0","SIMATIC WinCC RT Prof V15.1, upgrade WinCC V7.0..V7.4 RT/RC 64k-256k PowerTags -> WinCC Runtime Professional 64k-256k PowerTags V15.1, runtime software in TIA Portal, single license, SW and license key download, Class A, 5 languages (de,en,fr,es,it), executable in Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit) ******************************* E-mail address required for delivery",2657,"ST",1,"SIMATIC",1E-3,1,"6AV21054MM050AK0"]
["6AV2107-0CR00-0BB0","SIMATIC WinCC Sm@rtServer for SIMATIC Basic Panels, option for WinCC as of V14; Runtime software in TIA Portal; Single License; Without software a. documentation; License key on USB flash drive; Class A ******************************* Content: 1x USB",178,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21070CR000BB0"]
["6AV2107-0CR00-0BH0","SIMATIC WinCC Sm@rtServer for SIMATIC Basic Panels, Option for WinCC ab V14: Runtime software in TIA Portal; Single License; License key for download; without software a. documentation; Class A; ******************************* E-mail address required for delivery",158,"ST",1,"SIMATIC",1E-3,1,"6AV21070CR000BH0"]
["6AV2107-0DB00-0AL0","SIMATIC WinCC RT Prof. Client Software Update Service (SUS); Within the framework of this contract, you will receive updated software versions for a period of one year, if it is not cancelled three months prior to its expiration. Period of delivery and performance: 1 year from date of invoice. Prerequisite for contract: Current version of the client",619,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21070DB000AL0"]
["6AV2107-0DB00-0AY0","SIMATIC WinCC RT Prof. Client Software Update Service (SUS); Software Update Service, Within the framework of this contract, you will receive updated software versions for a period of one year, if it is not cancelled three months prior to its expiration. Period of delivery and performance: 1 year from date of invoice. Prerequisite for contract: Current version of the Client ******************************* email address is mandatory for delivery",578,"ST",1,"SIMATIC",1E-3,1,"6AV21070DB000AY0"]
["6AV2107-0DB05-0AA0","SIMATIC WinCC client for Runtime Prof. V15.1 runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit)/ ******************************* Content: Set (1x DVD + 1x USB)",2539,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21070DB050AA0"]
["6AV2107-0DB05-0AH0","SIMATIC WinCC Client for Runtime Professional V15.1 Runtime software in TIA Portal, Single license, software and documentation download, License key download, Class A, 5 languages (de, en, fr, es, it) executable under Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit) ******************************* E-mail address required for delivery",2258,"ST",1,"SIMATIC",1E-3,1,"6AV21070DB050AH0"]
["6AV2107-0DB15-0AA0","SIMATIC WinCC client for Runtime Prof. Asia V15.1 runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 6 languages (de,en,fr,es,it,zh), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit)/ ******************************* Content: Set (1x DVD + 1x USB)",2539,"ST",1,"SIMATIC",0.20200000000000001,1,"6AV21070DB150AA0"]
["6AV2107-0EB00-0BB0","SIMATIC WinCC Server for Runtime Professional Option for WinCC (TIA Portal) runtime software, single license without SW, without documentation License key on USB flash drive, Class A ******************************* Content: 1x USB",3712,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21070EB000BB0"]
["6AV2107-0EB00-0BH0","SIMATIC WinCC Server for Runtime Professional Option for WinCC (TIA Portal) License key download, single license for 1 installation R-SW, without SW and docu., Class A ******************************* E-mail address required for delivery",3302,"ST",1,"SIMATIC",1E-3,1,"6AV21070EB000BH0"]
["6AV2107-0FB00-0BB0","SIMATIC WinCC Redundancy for Runtime Professional V13 or higher Option for WinCC (TIA Portal) runtime software, Single license for 2 installations without SW, without documentation License key on USB flash drive, Class A ******************************* Content: 1x USB",3720,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21070FB000BB0"]
["6AV2107-0FB00-0BH0","SIMATIC WinCC Redundancy for Runtime Professional V13 or higher Option for WinCC (TIA Portal) License key download, Single license for 2 installations R-SW, without SW and docu., Class A ******************************* E-mail address required for delivery",3308,"ST",1,"SIMATIC",1E-3,1,"6AV21070FB000BH0"]
["6AV2107-0GA00-0BB0","SIMATIC WinCC Logging for Runtime Advanced option for WinCC (TIA Portal) runtime software, single license without SW, without documentation license key on USB flash drive, Class A ******************************* Content: 1x USB",297,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21070GA000BB0"]
["6AV2107-0GA00-0BH0","SIMATIC WinCC Logging for Runtime Advanced Option for WinCC (TIA Portal) License key download, single license for 1 installation R-SW, without SW and docu., Class A ******************************* E-mail address required for delivery",263,"ST",1,"SIMATIC",1E-3,1,"6AV21070GA000BH0"]
["6AV2107-0GA00-0BQ0","EPL Royalty for SIMATIC WinCC Logging for Runtime Advanced; only valid in connection with Enterprise License contract, requires EPL Master",290,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21070GA000BQ0"]
["6AV2107-0GB00-0BB0","SIMATIC WinCC Logging for Runtime Professional 1500 logging tags Option for WinCC (TIA Portal) runtime software, single license without SW, without documentation License key on USB flash drive, Class A ******************************* Content: 1x USB",2908,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21070GB000BB0"]
["6AV2107-0GB00-0BH0","SIMATIC WinCC Logging for Runtime Professional 1500 logging tags Option for WinCC (TIA Portal) License key download, single license for 1 installation R-SW, without SW and docu., Class A ******************************* E-mail address required for delivery",2587,"ST",1,"SIMATIC",1E-3,1,"6AV21070GB000BH0"]
["6AV2107-0GD00-0BB0","SIMATIC WinCC Logging for Runtime Professional 5000 logging tags Option for WinCC (TIA Portal) runtime software, single license without SW, without documentation License key on USB flash drive, Class A ******************************* Content: 1x USB",9738,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21070GD000BB0"]
["6AV2107-0GD00-0BH0","SIMATIC WinCC Logging for Runtime Professional 5000 Logging-Tags Option for WinCC (TIA Portal) License key download, single license for 1 installation R-SW, without SW and docu., Class A ******************************* E-mail address required for delivery",8660,"ST",1,"SIMATIC",1E-3,1,"6AV21070GD000BH0"]
["6AV2107-0HA00-0BB0","SIMATIC WinCC Recipes+Logging for Runtime Advanced option for WinCC (TIA Portal) runtime software, single license without SW, without documentation license key on USB flash drive, Class A ******************************* Content: 1x USB",465,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21070HA000BB0"]
["6AV2107-0HA00-0BH0","SIMATIC WinCC Recipes+Logging for Runtime Advanced Option for WinCC (TIA Portal) License key download, Single license, R-SW, without SW and docu., Class A ******************************* E-mail address required for delivery",420,"ST",1,"SIMATIC",1E-3,1,"6AV21070HA000BH0"]
["6AV2107-0HA00-0BQ0","EPL Royalty for SIMATIC WinCC Recipes+Logging for Runtime Advanced; only valid in connection with Enterprise License contract, requires EPL Master",455,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21070HA000BQ0"]
["6AV2107-0JA00-0BB0","SIMATIC WinCC Recipes for Runtime Advanced option for WinCC (TIA Portal) runtime software, single license without SW, without documentation license key on USB flash drive, Class A ******************************* Content: 1x USB",297,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21070JA000BB0"]
["6AV2107-0JA00-0BH0","SIMATIC WinCC Recipes for Runtime Advanced Option for WinCC (TIA Portal) License key download, single license for 1 installation R-SW, without SW and docu., Class A ******************************* E-mail address required for delivery",263,"ST",1,"SIMATIC",1E-3,1,"6AV21070JA000BH0"]
["6AV2107-0JA00-0BQ0","EPL Royalty for SIMATIC WinCC Recipes for Runtime Advanced; only valid in connection with Enterprise License contract, requires EPL Master",290,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21070JA000BQ0"]
["6AV2107-0JB00-0BB0","SIMATIC WinCC Recipes for Runtime Professional Option for WinCC (TIA Portal) runtime software, single license without SW, without documentation License key on USB flash drive, Class A ******************************* Content: 1x USB",918,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21070JB000BB0"]
["6AV2107-0JB00-0BH0","SIMATIC WinCC Recipes for Runtime Professional Option for WinCC (TIA Portal) License key download, single license for 1 installation R-SW, without SW and docu., Class A ******************************* E-mail address required for delivery",816,"ST",1,"SIMATIC",1E-3,1,"6AV21070JB000BH0"]
["6AV2107-0PX00-0AL0","SIMATIC Visualization Architect Software Update Service (SUS); Within the framework of this contract, you will receive for one year all up-to-date software versions. The contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice; Requirement for conclusion: current version of the software",847,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21070PX000AL0"]
["6AV2107-0PX00-0AQ0","EPL Royalty for SIMATIC Visualization Architect, only valid in connection with Enterprise License contract, requires EPL Master",4148,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21070PX000AQ0"]
["6AV2107-0PX00-0AR0","EPL Royalty for SIMATIC Visualization Architect, Payment for maintenance of a Royalty for 12 months, only valid in connection with Enterprise License contract, requires EPL Master",788,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21070PX000AR0"]
["6AV2107-0PX00-0AY0","SIMATIC Visualization Architect Software Update Service (SUS); Within the framework of this contract, you will receive for one year all up-to-date software versions. The contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice; Requirement for conclusion: current version of the software ******************************* E-mail address required for delivery",786,"ST",1,"SIMATIC",1E-3,1,"6AV21070PX000AY0"]
["6AV2107-0PX05-0AA5","SIMATIC Visualization Architect V15.1; Engineering software in TIA Portal; Floating License; Software and documentation on CD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh. ******************************* Content: Set (1x DVD + 1x USB)",4231,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21070PX050AA5"]
["6AV2107-0PX05-0AA6","SIMATIC Visualization Architect V15.1, 90-day Rental License; Engineering software in TIA Portal; Software and documentation on CD, License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh. ******************************* Content: Set (1x DVD + 1x USB)",1131,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21070PX050AA6"]
["6AV2107-0PX05-0AA7","SIMATIC Visualization Architect Trial V15.1; Engineering software in TIA Portal; Trial License; Software and documentation on CD; Class A; 6 languages: de,en,fr,es,it,zh. ******************************* Content: 1x DVD",27.900000000000002,"ST",1,"SIMATIC",0.191,1,"6AV21070PX050AA7"]
["6AV2107-0PX05-0AH5","SIMATIC Visualization Architect V15; Engineering software in TIA Portal; floating license; software, documentation and License key for download; Class A; 6 languages: de,en,fr,es,it,zh; ******************************* E-mail address required for delivery",3927,"ST",1,"SIMATIC",1E-3,1,"6AV21070PX050AH5"]
["6AV2107-0PX05-0AH6","SIMATIC Visualization Architect V15, 90-day Rental License; Engineering software in TIA Portal; software, documentation and license key for download; Class A; 6 languages: de,en,fr,es,it,zh; ******************************* E-mail address required for delivery",1008,"ST",1,"SIMATIC",1E-3,1,"6AV21070PX050AH6"]
["6AV2107-0RA00-0BB0","SIMATIC WinCC Audit for Runtime Advanced option for WinCC (TIA Portal) runtime software, single license without SW, without documentation license key on USB flash drive, Class A ******************************* Content: 1x USB",805,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21070RA000BB0"]
["6AV2107-0RA00-0BH0","SIMATIC WinCC Audit for Runtime Advanced Option for WinCC (TIA Portal) License key download, single license for 1 installation R-SW, without SW and docu., Class A ******************************* E-mail address required for delivery",714,"ST",1,"SIMATIC",1E-3,1,"6AV21070RA000BH0"]
["6AV2107-0RA00-0BQ0","EPL Royalty for SIMATIC WinCC Audit for Runtime Advanced; only valid in connection with Enterprise License contract, requires EPL Master",789,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21070RA000BQ0"]
["6AV2107-0RP00-0BB0","SIMATIC WinCC Audit for SIMATIC Comfort/Mobile Panels option for WinCC (TIA Portal) runtime software, single license without SW, without documentation license key on USB flash drive, Class A ******************************* Content: 1x USB",533,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21070RP000BB0"]
["6AV2107-0RP00-0BH0","SIMATIC WinCC Audit for SIMATIC Comfort/Mobile Panels Option for WinCC (TIA Portal) License key download, single license for 1 installation R-SW, without SW and docu., Class A ******************************* E-mail address required for delivery",473,"ST",1,"SIMATIC",1E-3,1,"6AV21070RP000BH0"]
["6AV2107-0UA00-0BB0","SIMATIC ProDiag for WinCC Runtime Advanced, Controls for WinCC V14 or higher; Runtime software in TIA Portal; Single License; Without software a. documentation; License key on USB flash drive; Class A ******************************* Content: 1x USB",885,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21070UA000BB0"]
["6AV2107-0UA00-0BH0","SIMATIC ProDiag for WinCC Runtime Advanced, Controls for WinCC V14 or higher; Runtime software in TIA Portal; Single License; License key for download; without software a. documentation; Class A; ******************************* E-mail address required for delivery",788,"ST",1,"SIMATIC",1E-3,1,"6AV21070UA000BH0"]
["6AV2107-0UA00-0BQ0","EPL Royalty for SIMATIC ProDiag for WinCC Runtime Advanced; only valid in connection with Enterprise License contract, requires EPL Master",867,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21070UA000BQ0"]
["6AV2107-0UB00-0BB0","SIMATIC ProDiag for WinCC Runtime Professional Controls for WinCC V14 or higher; Runtime software in TIA Portal; Single License; without software a. documentation; license key on USB stick; Class A dasfjfgggrg ******************************* Content: 1x USB",1002,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21070UB000BB0"]
["6AV2107-0UB00-0BH0","SIMATIC ProDiag for WinCC Runtime Professional Controls for WinCC V14 or higher; Runtime software in TIA Portal; Single License; without software a. documentation; License key for download; Class A ***************************** ** E-mail address required for delivery",893,"ST",1,"SIMATIC",1E-3,1,"6AV21070UB000BH0"]
["6AV2107-0UP00-0BB0","SIMATIC ProDiag for SIMATIC Comfort/Mobile Panels, Controls for WinCC V14 or higher; Runtime software in TIA Portal; Single License; Without software a. documentation; License key on USB flash drive; Class A ******************************* Content: 1x USB",590,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21070UP000BB0"]
["6AV2107-0UP00-0BH0","SIMATIC ProDiag for SIMATIC Comfort/Mobile Panels, Controls for WinCC V14 or higher; Runtime software in TIA Portal; Single License; License key for download; without software a. documentation; Class A; ******************************* E-mail address required for delivery",525,"ST",1,"SIMATIC",1E-3,1,"6AV21070UP000BH0"]
["6AV2107-2GD00-0BD0","SIMATIC WinCC Logging for Runtime Professional Powerpack 1500-> 5000 logging tags Option for WinCC (TIA Portal) runtime software, single license without SW, without documentation License key on USB flash drive, Class A ******************************* Content: 1x USB",6830,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21072GD000BD0"]
["6AV2107-2GD00-0BJ0","SIMATIC WinCC Logging for Runtime Professional Power Pack 1500-> 5000 Logging-Tags Option for WinCC (TIA Portal) License key download, single license for 1 installation R-SW, without SW and docu., Class A ******************************* E-mail address required for delivery",6073,"ST",1,"SIMATIC",1.4999999999999999E-2,1,"6AV21072GD000BJ0"]
["6AV2107-3DB05-0AE0","SIMATIC WinCC client for Runtime Prof. V15.1 Upgrade V11..V14 -> V15.1, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit)/ ******************************* Content: Set (1x DVD + 1x USB)",1016,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21073DB050AE0"]
["6AV2107-3DB05-0AK0","SIMATIC WinCC Client for Runtime Prof. V15.1 Upgrade V11..V14 -> V15.1, Runtime software in TIA Portal, Single license, software and documentation download, License key download, Class A, 5 languages (de, en, fr, es, it) executable under Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit) ******************************* E-mail address required for delivery",903,"ST",1,"SIMATIC",1E-3,1,"6AV21073DB050AK0"]
["6AV2107-3PX05-0AA5","SIMATIC Visualization Architect V15.1, Upgrade V14 -> V15.1; Engineering software in TIA Portal; Software and documentation on CD, License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh. ******************************* Content: Set (1x DVD + 1x USB)",1693,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21073PX050AA5"]
["6AV2107-3PX05-0AH5","SIMATIC Visualization Architect V15, upgrade V14 -> V15; Engineering software in TIA Portal; software, documentation and license key for download; Class A; 6 languages: de,en,fr,es,it,zh; ******************************* E-mail address required for delivery",1571,"ST",1,"SIMATIC",1E-3,1,"6AV21073PX050AH5"]
["6AV2107-4DB05-0AE0","SIMATIC WinCC client for Runtime Prof. V15.1 UG WinCC V7.0..V7.4 RT/RC 128 / RC/RT Client-> WinCC Client for Runtime Prof. V15.1 runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult SP1 (64-bit)/ 10 Prof/Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 / 2016 (64-bit)/ ******************************* Content: Set (1x DVD + 1x USB)",1016,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21074DB050AE0"]
["6AV2107-4DB05-0AK0","SIMATIC WinCC Client for Runtime Prof. V15.1 UG WinCC V7.0..V7.4 RT/RC 128 / RC/RT Client-> WinCC Client for Runtime Prof. V15.1 Runtime software in TIA Portal, Single license, Software and License key download, Class A, 5 languages (de, en, fr, es, it) executable under Windows 7 Prof/Ent/Ult SP1 (64 bit)/ 10 Prof/Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 / 2016 (64 bit/ ******************************* E-mail address required for delivery",903,"ST",1,"SIMATIC",1E-3,1,"6AV21074DB050AK0"]
["6AV2107-4GX00-0BF0","SIMATIC WinCC Logging Upgrade for SIMATIC WinCC Archives V7.0 Option for WinCC (TIA Portal) runtime software, single license without SW, without documentation 10 license keys on USB flash drive, Class A ******************************* Content: 1x USB",38.4,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21074GX000BF0"]
["6AV2107-4GX00-0BK0","SIMATIC WinCC Logging Upgrade for SIMATIC WinCC Archives V7.0 Option for WinCC (TIA Portal) License key download, Single license, R-SW, without SW and docu., Class A ******************************* E-mail address required for delivery",34.200000000000003,"ST",1,"SIMATIC",1E-3,1,"6AV21074GX000BK0"]
["6AV2107-4XP00-0BF0","SIMATIC WinCC Panel Options Upgrade for WinCC flexible Panel Options (Sm@rtAccess/ SM@RTSERVICE/Audit) option for WinCC (TIA Portal) runtime software, single license without SW, without documentation license key on USB flash drive, Class A ******************************* Content: 1x USB",35.5,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21074XP000BF0"]
["6AV2107-4XP00-0BK0","SIMATIC WinCC Panel Options Upgrade for WinCC flexible Panel options (Sm@rtAccess/ SM@RTSERVICE/Audit) Option for WinCC (TIA Portal) License key download, Single license, R-SW, without SW and docu., Class A ******************************* E-mail address required for delivery",31.5,"ST",1,"SIMATIC",1E-3,1,"6AV21074XP000BK0"]
["6AV2107-8PX03-0AP0","EPL master for SIMATIC Visualization Architect V15.1 (EPL=Enterprise License); Mandatory royalty per 1 installation; Only valid in connection with Enterprise License contract",314,"ST",1,"SIMATIC",0.224,1,"6AV21078PX030AP0"]
["6AV2108-0AA00-0AL0","SIMATIC Energy Suite Engineering, Software Update Service; Within the framework of this contract, you will receive for one year all up-to-date software versions. The contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice; Requirement for conclusion: current version of the software",142,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21080AA000AL0"]
["6AV2108-0AA00-0AY0","SIMATIC Energy Suite Engineering, Software Update Service; Within the framework of this contract, you will receive for one year all up-to-date software versions. The contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice; Requirement for conclusion: current version of the software ******************************* E-mail address required for delivery",126,"ST",1,"SIMATIC",1E-3,1,"6AV21080AA000AY0"]
["6AV2108-0AA05-0AA5","SIMATIC Energy Suite V15.1, Engineering software in TIA Portal; Floating License; SW and documentation on CD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; contains license certificate for 10 energy objects (2x5 EnO) ******************************* Content: Set (1x DVD + 1x USB)",943,"ST",1,"SIMATIC",0.219,1,"6AV21080AA050AA5"]
["6AV2108-0AA05-0AA7","SIMATIC Energy Suite Trial V15.1, engineering software in TIA Portal; Trial License; SW and documentation on CD; Class A; 6 languages: de,en,fr,es,it,zh; ******************************* Content: 1x DVD",27.900000000000002,"ST",1,"SIMATIC",0.191,1,"6AV21080AA050AA7"]
["6AV2108-0AA05-0AH5","SIMATIC Energy Suite V15, Engineering software in the TIA Portal; floating license; software, documentation and License key for download; Class A; 6 languages: de,en,fr,es,it,zh; contains license certificate for 10 energy objects (2x5 EnO) as pdf for download ******************************* E-mail address required for delivery",840,"ST",1,"SIMATIC",1E-3,1,"6AV21080AA050AH5"]
["6AV2108-0CF00-0BB0","SIMATIC Energy Suite S7-1500, Single Runtime License; contains license certificate for 5 energy objects (1x5 EnO); Class A, executable on all S7-1500 CPU (without S7-1500S) and ET 200SP CPU Firmware V2.0 or higher",236,"ST",1,"SIMATIC",8.9999999999999993E-3,1,"6AV21080CF000BB0"]
["6AV2108-0CF00-0BH0","SIMATIC Energy Suite S7-1500, Single Runtime License Download contains license certificate for 5 energy objects (1x5 EnO) as pdf for download, Class A; executable on all S7-1500 CPU (without S7-1500S) and ET 200SP CPU Firmware V2.0 or higher ******************************* E-mail address required for delivery",210,"ST",1,"SIMATIC",1E-3,1,"6AV21080CF000BH0"]
["6AV2108-0CH00-0BB0","SIMATIC Energy Suite S7-1500, Single Runtime License; contains license certificate for 10 energy objects (1x10 EnO); Class A, executable on all S7-1500 CPU (without S7-1500S) and ET 200SP CPU Firmware V2.0 or higher",472,"ST",1,"SIMATIC",8.9999999999999993E-3,1,"6AV21080CH000BB0"]
["6AV2108-0CH00-0BH0","SIMATIC Energy Suite S7-1500, Single Runtime License Download contains license certificate for 10 energy objects (1x10 EnO) as pdf for download, Class A; executable on all S7-1500 CPU (without S7-1500S) and ET 200SP CPU Firmware V2.0 or higher ******************************* E-mail address required for delivery",420,"ST",1,"SIMATIC",1E-3,1,"6AV21080CH000BH0"]
["6AV2108-0DF00-0BB0","SIMATIC Energy Suite S7-1500, Single Runtime License; contains license certificate for 10 energy objects (2x5 EnO); Class A, executable on all S7-1500 CPU (without S7-1500S) and ET 200SP CPU Firmware V2.0 or higher",472,"ST",1,"SIMATIC",0.1,1,"6AV21080DF000BB0"]
["6AV2108-0DF00-0BH0","SIMATIC Energy Suite S7-1500, Single Runtime License Download contains license certificate for 10 energy objects (2x5 EnO) as pdf for download, Class A; executable on all S7-1500 CPU (without S7-1500S) and ET 200SP CPU Firmware V2.0 or higher ******************************* E-mail address required for delivery",420,"ST",1,"SIMATIC",1E-3,1,"6AV21080DF000BH0"]
["6AV2108-0FH00-0BB0","SIMATIC Energy Suite S7-1500, Single Runtime License; contains license certificate for 50 energy objects (5x10 EnO); Class A, executable on all S7-1500 CPU (without S7-1500S) and ET 200SP CPU Firmware V2.0 or higher",2357,"ST",1,"SIMATIC",0.1,1,"6AV21080FH000BB0"]
["6AV2108-0FH00-0BH0","SIMATIC Energy Suite S7-1500, Single Runtime License Download contains license certificate for 50 energy objects (5x10 EnO) as pdf for download, Class A; executable on all S7-1500 CPU (without S7-1500S) and ET 200SP CPU Firmware V2.0 or higher ******************************* E-mail address required for delivery",2100,"ST",1,"SIMATIC",1E-3,1,"6AV21080FH000BH0"]
["6AV2108-0HH00-0BB0","SIMATIC Energy Suite S7-1500, Single Runtime License; contains license certificate for 100 energy objects (10x10 EnO); Class A, executable on all S7-1500 CPU (without S7-1500S) and ET 200SP CPU Firmware V2.0 or higher",4713,"ST",1,"SIMATIC",0.1,1,"6AV21080HH000BB0"]
["6AV2108-0HH00-0BH0","SIMATIC Energy Suite S7-1500, Single Runtime License Download contains license certificate for 100 energy objects (10x10 EnO) as pdf for download, Class A; executable on all S7-1500 CPU (without S7-1500S) and ET 200SP CPU Firmware V2.0 or higher ******************************* E-mail address required for delivery",4200,"ST",1,"SIMATIC",1E-3,1,"6AV21080HH000BH0"]
["6AV2108-1CF00-0BB0","S7 Energy Efficiency Monitor for machines S7-1500/1200; Single Runtime License; contains license certificate for Machines S7-1500/1200; Class A, can be executed on: S7-1500 CPU Firmware V2.1 or higher, ET 200SP CPU Firmware V2.1 or higher, S7-1200 CPU Firmware V4.2 or higher",236,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21081CF000BB0"]
["6AV2108-1CF00-0BH0","S7 Energy Efficiency Monitor for machines, S7-1500/1200; Single Runtime License Download contains license certificate for machines S7-1500/1200; as PDF for download, class A; can execute on: S7-1500 CPU as of firmware V2.1, ET 200SP CPU Firmware V2.1, or higher S7-1200 CPU as of firmware V4.2 ******************************* E-mail address required for delivery",210,"ST",1,"SIMATIC",1E-3,1,"6AV21081CF000BH0"]
["6AV2108-3AA05-0AE5","SIMATIC Energy Suite V15.1, Upgrade V14 -> V15.1; Engineering software in TIA Portal; Floating License; SW and documentation on CD; License key on USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; ******************************* Content: Set (1x DVD + 1x USB)",283,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV21083AA050AE5"]
["6AV2108-3AA05-0AK5","SIMATIC Energy Suite V15, upgrade V14 -> V15; Engineering software in the TIA Portal; floating license; software, documentation and License key for download; Class A; 6 languages: de,en,fr,es,it,zh. ******************************* E-mail address required for delivery",252,"ST",1,"SIMATIC",1E-3,1,"6AV21083AA050AK5"]
["6AV2112-5AA01-0AA5","Solution Partner SIMATIC HMI SIMATIC WinCC Advanced Basic software package, Consisting of: SIMATIC WinCC Advanced",880,"ST",1,"SIMATIC",0.221,1,"6AV21125AA010AA5"]
["6AV2113-8XA00-0YQ0","SIMATIC WinCC Professional max. Power Tags V15, EPL royalty; Royalty for 1 installation; only valid in connection with Enterprise license contract: 00011-GB8; requires EPL Master",4200,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21138XA000YQ0"]
["6AV2113-8XA00-0YQ1","SIMATIC WinCC Professional max. Power Tags V15, EPL royalty for service; Royalty for 1 installation; only valid in connection with Enterprise license contract: 00011-GB8; requires EPL Master",4200,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21138XA000YQ1"]
["6AV2114-2BA05-0AA0","SIMATIC WinCC Runtime Advanced SW package for SIMATIC IPC, 128 power tags; includes: WinCC Runtime Advanced 128 PowerTags V15.1, SIMATIC WinCC Recipes+Logging for Runtime Advanced; Supply only if the same number of SIMATIC IPCs is ordered.",378,"ST",1,"SIMATIC",0.36499999999999999,1,"6AV21142BA050AA0"]
["6AV2114-2DA05-0AA0","SIMATIC WinCC Runtime Advanced SW package for SIMATIC IPC, 512 power tags; includes: WinCC Runtime Advanced 512 PowerTags V15.1, SIMATIC WinCC Recipes+Logging for Runtime Advanced; Supply only if the same number of SIMATIC IPCs is ordered.",1230,"ST",1,"SIMATIC",0.36499999999999999,1,"6AV21142DA050AA0"]
["6AV2114-2FA05-0AA0","SIMATIC WinCC Runtime Advanced SW package for SIMATIC IPC, 2048 power tags; includes: WinCC Runtime Advanced 2048 PowerTags V15.1, SIMATIC WinCC Recipes+Logging for Runtime Advanced; Supply only if the same number of SIMATIC IPCs is ordered.",1890,"ST",1,"SIMATIC",0.36499999999999999,1,"6AV21142FA050AA0"]
["6AV2114-2HA05-0AA0","SIMATIC WinCC Runtime Advanced SW package for SIMATIC IPC, 4096 power tags; includes: WinCC Runtime Advanced 4096 PowerTags V15.1, SIMATIC WinCC Recipes+Logging for Runtime Advanced; Supply only if the same number of SIMATIC IPCs is ordered.",2835,"ST",1,"SIMATIC",0.36499999999999999,1,"6AV21142HA050AA0"]
["6AV2114-2KA05-0AA0","SIMATIC WinCC Runtime Advanced SW package for SIMATIC IPC, 8192 power tags; includes: WinCC Runtime Advanced 8192 PowerTags V15.1, SIMATIC WinCC Recipes+Logging for Runtime Advanced; Supply only if the same number of SIMATIC IPCs is ordered.",3779,"ST",1,"SIMATIC",0.36499999999999999,1,"6AV21142KA050AA0"]
["6AV2115-2BA05-0AA0","WinCC Runtime Professional software package for SIMATIC IPC, 128 PowerTags, includes: WinCC Runtime Professional 128 PowerTags V15.1; Supply only if the same number of SIMATIC IPCs is ordered. ******************************* Content: 6AV2105-0BA05-0AA0",2150,"ST",1,"SIMATIC",0.2,1,"6AV21152BA050AA0"]
["6AV2115-2DA05-0AA0","WinCC Runtime Professional software package for SIMATIC IPC, 512 PowerTags, includes: WinCC Runtime Professional 512 PowerTags V15.1; Supply only if the same number of SIMATIC IPCs is ordered. ******************************* Content: 6AV2105-0DA05-0AA0",3288,"ST",1,"SIMATIC",0.2,1,"6AV21152DA050AA0"]
["6AV2115-2FA05-0AA0","WinCC Runtime Professional software package for SIMATIC IPC, 2048 PowerTags, includes: WinCC Runtime Professional 2048 PowerTags V15.1; Supply only if the same number of SIMATIC IPCs is ordered. ******************************* Content: 6AV2105-0FA05-0AA0",4047,"ST",1,"SIMATIC",0.2,1,"6AV21152FA050AA0"]
["6AV2115-2HA05-0AA0","WinCC Runtime Professional software package for SIMATIC IPC, 4096 PowerTags, includes: WinCC Runtime Professional 4096 PowerTags V15.1; Supply only if the same number of SIMATIC IPCs is ordered. ******************************* Content: 6AV2105-0HA05-0AA0",4452,"ST",1,"SIMATIC",0.2,1,"6AV21152HA050AA0"]
["6AV2115-2KA05-0AA0","WinCC Runtime Professional software package for SIMATIC IPC, 8192 PowerTags, includes: WinCC Runtime Professional 8192 PowerTags V15.1; Supply only if the same number of SIMATIC IPCs is ordered. ******************************* Content: 6AV2105-0KA05-0AA0",4858,"ST",1,"SIMATIC",0.2,1,"6AV21152KA050AA0"]
["6AV2115-2MA05-0AA0","WinCC Runtime Professional software package for SIMATIC IPC, 65536 PowerTags, includes: WinCC Runtime Professional 65536 PowerTags V15.1; Supply only if the same number of SIMATIC IPCs is ordered. ******************************* Content: 6AV2105-0MA05-0AA0",5969,"ST",1,"SIMATIC",0.2,1,"6AV21152MA050AA0"]
["6AV2117-0CP00-0BB0","SIMATIC WinCC SM@RT Server for SIMATIC Panels, Option for WinCC (TIA Portal), runtime software, Single license, without SW, without documentation, Class A, only license",328,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21170CP000BB0"]
["6AV2117-0PX00-0AA5","Solution Partner SIMATIC HMI SIMATIC Visualization Architect consisting of: SIMATIC Visualization Architect Engineering software in TIA Portal; floating license; Software and documentation on CD; License key on a USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh.",1983,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV21170PX000AA5"]
["6AV2117-2DB05-0AA0","WinCC Client for RT Prof. software package for SIMATIC IPC; includes: WinCC Client for Runtime Professional V15.1; Supply only if the same number of SIMATIC IPCs is ordered. ******************************* Content: 6AV2107-0DB05-0AA0",2031,"ST",1,"SIMATIC",0.2,1,"6AV21172DB050AA0"]
["6AV2117-8PX03-0YQ0","SIMATIC Visualization Architect V15; EPL royalty; Royalty for 1 installation; only valid in connection with Enterprise license contract: 00011-GB8; requires EPL Master",2310,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21178PX030YQ0"]
["6AV2117-8PX03-0YQ1","SIMATIC Visualization Architect V15; EPL royalty for service; Royalty for 1 installation; only valid in connection with Enterprise license contract: 00011-GB8; requires EPL Master",2310,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV21178PX030YQ1"]
["6AV2123-2DB03-0AA0","training pack KTP400 Basic/XB005, Consisting of: 6xKTP400 Basic, 6xSCALANCE XB005 unmanaged IE switch, 12x RJ45 cable, Length 6m, 6xWinCC Basic (TIA Portal) ******************************* for educational purposes only",2769,"ST",1,"SIMATIC",8,1,"6AV21232DB030AA0"]
["6AV2123-2DB03-0AA1","training pack KTP400 Basic/XB005, Consisting of: 1x KTP400 Basic, 1x SCALANCE XB005 unmanaged IE switch, 2x RJ45 cables, Length 6m, 1x WinCC Basic (TIA Portal) ******************************* for educational purposes only",485,"ST",1,"SIMATIC",1.5,1,"6AV21232DB030AA1"]
["6AV2123-2DB03-0AX0","SIMATIC HMI, KTP400 Basic, Basic Panel, Key/touch operation, 4\" TFT display, 65536 colors, PROFINET interface, configurable from WinCC Basic V13/ STEP 7 Basic V13, contains open-source software, which is provided free of charge see enclosed CD",361,"ST",1,"SIMATIC",0.45900000000000002,1,"6AV21232DB030AX0"]
["6AV2123-2GA03-0AX0","SIMATIC HMI, KTP700 Basic DP, Basic Panel, Key/touch operation, 7\" TFT display, 65536 colors, PROFIBUS interface, configurable as of WinCC Basic V13/ STEP 7 Basic V13, contains open-source software, which is provided free of charge see enclosed CD",656,"ST",1,"SIMATIC",0.8,1,"6AV21232GA030AX0"]
["6AV2123-2GB03-0AA0","training pack KTP700 Basic/XB005, Consisting of: 6xKTP700 Basic, 6xSCALANCE XB005 unmanaged IE switch, 12x RJ45 cable, Length 6m, configurable from WinCC Basic V13/ STEP 7 Basic V13, contains open-source software, which is provided free of charge see enclosed CD ******************************* for educational purposes only",3096,"ST",1,"SIMATIC",2,1,"6AV21232GB030AA0"]
["6AV2123-2GB03-0AA1","training pack KTP700 Basic/XB005, Consisting of: 1x KTP700 Basic, 1x SCALANCE XB005 unmanaged IE switch, 2x RJ45 cables, Length 6m, configurable from WinCC Basic V13/ STEP 7 Basic V13, contains open-source software, which is provided free of charge see enclosed CD ******************************* for educational purposes only",665,"ST",1,"SIMATIC",10,1,"6AV21232GB030AA1"]
["6AV2123-2GB03-0AX0","SIMATIC HMI, KTP700 Basic, Basic Panel, Key/touch operation, 7\" TFT display, 65536 colors, PROFINET interface, configurable from WinCC Basic V13/ STEP 7 Basic V13, contains open-source software, which is provided free of charge see enclosed CD",656,"ST",1,"SIMATIC",0.97699999999999998,1,"6AV21232GB030AX0"]
["6AV2123-2JB03-0AX0","SIMATIC HMI, KTP900 Basic, Basic Panel, Key/touch operation, 9\" TFT display, 65536 colors, PROFINET interface, configurable from WinCC Basic V13/ STEP 7 Basic V13, contains open-source software, which is provided free of charge see enclosed CD",1148,"ST",1,"SIMATIC",1.1299999999999999,1,"6AV21232JB030AX0"]
["6AV2123-2MA03-0AX0","SIMATIC HMI, KTP1200 Basic DP, Basic Panel, Key/touch operation, 12\" TFT display, 65536 colors, PROFIBUS interface, configurable as of WinCC Basic V13/ STEP 7 Basic V13, contains open-source software, which is provided free of charge see enclosed CD",1640,"ST",1,"SIMATIC",2.17,1,"6AV21232MA030AX0"]
["6AV2123-2MB03-0AX0","SIMATIC HMI, KTP1200 Basic, Basic Panel, Key/touch operation, 12\" TFT display, 65536 colors, PROFINET interface, configurable from WinCC Basic V13/ STEP 7 Basic V13, contains open-source software, which is provided free of charge see enclosed CD",1640,"ST",1,"SIMATIC",2.1619999999999999,1,"6AV21232MB030AX0"]
["6AV2124-0GC01-0AX0","SIMATIC HMI TP700 Comfort, Comfort Panel, Touch operation, 7\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 12 MB configuration memory, Windows CE 6.0 (Microsoft Support included Security updates discontinued) configurable from WinCC Comfort V11",1120,"ST",1,"SIMATIC",1.5349999999999999,1,"6AV21240GC010AX0"]
["6AV2124-0GC10-0SA0","Starter package TP700 Outdoor incl. Outdoor SD Card, Touch pen system and engineering system, most current version of WinCC Comfort",1890,"ST",1,"SIMATIC",1.94,1,"6AV21240GC100SA0"]
["6AV2124-0GC13-0AX0","SIMATIC HMI TP700 Comfort Outdoor, Comfort Panel, Touch operation, 7\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 12 MB configuration memory, Windows CE 6.0 (Microsoft Support included Security updates discontinued) configurable from WinCC Comfort V13 SP1, HSP",1607,"ST",1,"SIMATIC",1.819,1,"6AV21240GC130AX0"]
["6AV2124-0JC01-0AX0","SIMATIC HMI TP900 Comfort, Comfort Panel, Touch operation, 9\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 12 MB configuration memory, Windows CE 6.0, (Microsoft Support included Security updates discontinued) configurable from WinCC Comfort V11",1923,"ST",1,"SIMATIC",2.5259999999999998,1,"6AV21240JC010AX0"]
["6AV2124-0MC01-0AX0","SIMATIC HMI TP1200 Comfort, Comfort Panel, Touch operation, 12\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 12 MB configuration memory, Windows CE 6.0 (Microsoft Support included Security updates discontinued) configurable from WinCC Comfort V11",2488,"ST",1,"SIMATIC",3.4620000000000002,1,"6AV21240MC010AX0"]
["6AV2124-0MC24-0AB0","SIMATIC HMI TP1200 Comfort Pro Support arm, neutral front, Comfort Panel, touch operation, 12\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 12 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",2785,"ST",1,"SIMATIC",5.923,1,"6AV21240MC240AB0"]
["6AV2124-0MC24-0AX0","SIMATIC HMI TP1200 Comfort Pro Support arm, Comfort Panel, touch operation, 12\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 12 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",2678,"ST",1,"SIMATIC",5.9139999999999997,1,"6AV21240MC240AX0"]
["6AV2124-0MC24-0BB0","SIMATIC HMI TP1200 Comfort Pro support arm for Extension Unit, neutral front, Comfort Panel, touch operation, 12\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 12 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",2785,"ST",1,"SIMATIC",5.9260000000000002,1,"6AV21240MC240BB0"]
["6AV2124-0MC24-0BX0","SIMATIC HMI TP1200 Comfort Pro support arm for Extension Unit, Comfort Panel, touch operation, 12\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 12 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",2678,"ST",1,"SIMATIC",5.97,1,"6AV21240MC240BX0"]
["6AV2124-0MC24-1AB0","SIMATIC HMI TP1200 Comfort Pro Supporting foot, neutral front, Comfort Panel, touch operation, 12\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 12 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",2785,"ST",1,"SIMATIC",5.8849999999999998,1,"6AV21240MC241AB0"]
["6AV2124-0MC24-1AX0","SIMATIC HMI TP1200 Comfort Pro Supporting foot, Comfort Panel, touch operation, 12\" widescreen TFT display 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 12 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",2678,"ST",1,"SIMATIC",5.8929999999999998,1,"6AV21240MC241AX0"]
["6AV2124-0QC02-0AX1","SIMATIC HMI TP1500 Comfort, Comfort Panel, Touch operation, 15\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",3166,"ST",1,"SIMATIC",5.56,1,"6AV21240QC020AX1"]
["6AV2124-0QC10-0SA0","Starter package TP1500 Outdoor incl. Outdoor SD Card, Touch pen system and engineering system, most current version of WinCC Comfort",4830,"ST",1,"SIMATIC",7.58,1,"6AV21240QC100SA0"]
["6AV2124-0QC13-0AX0","SIMATIC HMI TP1500 Comfort Outdoor, Comfort Panel, Touch operation, 15\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 12 MB configuration memory, Windows CE 6.0 (Microsoft Support included Security updates discontinued) configurable from WinCC Comfort V13 SP1, HSP",4463,"ST",1,"SIMATIC",5.42,1,"6AV21240QC130AX0"]
["6AV2124-0QC24-0AB0","SIMATIC HMI TP1500 Comfort Pro, support arm, neutral front, Comfort Panel, Touch operation, 15\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",3428,"ST",1,"SIMATIC",7.2450000000000001,1,"6AV21240QC240AB0"]
["6AV2124-0QC24-0AX0","SIMATIC HMI TP1500Comfort Pro, support arm, Comfort Panel, Touch operation, 15\"; widescreen TFT display 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",3321,"ST",1,"SIMATIC",7.2990000000000004,1,"6AV21240QC240AX0"]
["6AV2124-0QC24-0BB0","SIMATIC HMI TP1500 Comfort Pro, Support arm for Extension Unit, Neutral front, Comfort Panel, Touch operation, 15\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",3428,"ST",1,"SIMATIC",7.2450000000000001,1,"6AV21240QC240BB0"]
["6AV2124-0QC24-0BX0","SIMATIC HMI TP1500 Comfort Pro, Support arm for Extension Unit, Comfort Panel, Touch operation, 15\"; widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",3321,"ST",1,"SIMATIC",7.2750000000000004,1,"6AV21240QC240BX0"]
["6AV2124-0QC24-1AB0","SIMATIC HMI TP1500 Comfort Pro, stand, neutral front, Comfort Panel, Touch operation, 15\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",3428,"ST",1,"SIMATIC",7.2549999999999999,1,"6AV21240QC241AB0"]
["6AV2124-0QC24-1AX0","SIMATIC HMI TP1500 Comfort Pro, stand, Comfort Panel, Touch operation, 15\"; widescreen TFT display 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",3321,"ST",1,"SIMATIC",7.2610000000000001,1,"6AV21240QC241AX0"]
["6AV2124-0UC02-0AX1","SIMATIC HMI TP1900 Comfort, Comfort Panel, Touch operation, 19\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",3845,"ST",1,"SIMATIC",6.63,1,"6AV21240UC020AX1"]
["6AV2124-0UC24-0AB0","SIMATIC HMI TP1900 Comfort Pro, support arm, neutral front, Comfort Panel, Touch operation, 19\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",4177,"ST",1,"SIMATIC",8.84,1,"6AV21240UC240AB0"]
["6AV2124-0UC24-0AX0","SIMATIC HMI TP1900 Comfort Pro, support arm, Comfort Panel, Touch operation, 19\" widescreen TFT display 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",4070,"ST",1,"SIMATIC",8.84,1,"6AV21240UC240AX0"]
["6AV2124-0UC24-0BB0","SIMATIC HMI TP1900 Comfort Pro, Support arm for Extension Unit, Neutral front, Comfort Panel, Touch operation, 19\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",4177,"ST",1,"SIMATIC",8.86,1,"6AV21240UC240BB0"]
["6AV2124-0UC24-0BX0","SIMATIC HMI TP1900 Comfort Pro, Support arm for Extension Unit, Comfort Panel, Touch operation, 19\" widescreen TFT display 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",4070,"ST",1,"SIMATIC",8.84,1,"6AV21240UC240BX0"]
["6AV2124-0UC24-1AB0","SIMATIC HMI TP1900 Comfort Pro, stand, neutral front, Comfort Panel, Touch operation, 19\" widescreen TFT display 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",4177,"ST",1,"SIMATIC",8.7799999999999994,1,"6AV21240UC241AB0"]
["6AV2124-0UC24-1AX0","SIMATIC HMI TP1900 Comfort Pro, stand, Comfort Panel, Touch operation, 19\" widescreen TFT display 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",4070,"ST",1,"SIMATIC",8.8350000000000009,1,"6AV21240UC241AX0"]
["6AV2124-0XC02-0AX1","SIMATIC HMI TP2200 Comfort, Comfort Panel, Touch operation, 22\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",4512,"ST",1,"SIMATIC",8.1199999999999992,1,"6AV21240XC020AX1"]
["6AV2124-0XC24-0AB0","SIMATIC HMI TP2200 Comfort Pro, support arm, neutral front, Comfort Panel, touch operation, 22\" widescreen TFT display 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",4809,"ST",1,"SIMATIC",9.8800000000000008,1,"6AV21240XC240AB0"]
["6AV2124-0XC24-0AX0","SIMATIC HMI TP2200 Comfort Pro, support arm, Comfort Panel, Touch operation, 22\"; widescreen TFT display 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",4702,"ST",1,"SIMATIC",9.8800000000000008,1,"6AV21240XC240AX0"]
["6AV2124-0XC24-0BB0","SIMATIC HMI TP2200 Comfort Pro, Support arm for Extension Unit, Neutral front, Comfort Panel, Touch operation, 22\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",4809,"ST",1,"SIMATIC",9.9600000000000009,1,"6AV21240XC240BB0"]
["6AV2124-0XC24-0BX0","SIMATIC HMI TP2200 Comfort Pro, Support arm for Extension Unit, Comfort Panel, Touch operation, 22\"; widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",4702,"ST",1,"SIMATIC",9.98,1,"6AV21240XC240BX0"]
["6AV2124-0XC24-1AB0","SIMATIC HMI TP2200 Comfort Pro, pedestal, neutral front, Comfort Panel, touch operation, 22\" widescreen TFT display 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",4809,"ST",1,"SIMATIC",9.86,1,"6AV21240XC241AB0"]
["6AV2124-0XC24-1AX0","SIMATIC HMI TP2200 Comfort Pro, stand, Comfort Panel, Touch operation, 22\"; widescreen TFT display 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",4702,"ST",1,"SIMATIC",9.6999999999999993,1,"6AV21240XC241AX0"]
["6AV2124-1DC01-0AX0","SIMATIC HMI KP400 Comfort, Comfort Panel, key operation, 4\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 4 MB configuration memory, Windows CE 6.0, (Microsoft Support included Security updates discontinued) configurable from WinCC Comfort V11",679,"ST",1,"SIMATIC",0.85699999999999998,1,"6AV21241DC010AX0"]
["6AV2124-1GC01-0AX0","SIMATIC HMI KP700 Comfort, Comfort Panel, key operation, 7\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 12 MB configuration memory, Windows CE 6.0, (Microsoft Support included Security updates discontinued) configurable from WinCC Comfort V11",1233,"ST",1,"SIMATIC",2.738,1,"6AV21241GC010AX0"]
["6AV2124-1JC01-0AX0","SIMATIC HMI KP900 Comfort, Comfort Panel, key operation, 9\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 12 MB configuration memory, Windows CE 6.0, (Microsoft Support included Security updates discontinued) configurable from WinCC Comfort V11",2035,"ST",1,"SIMATIC",3.31,1,"6AV21241JC010AX0"]
["6AV2124-1MC01-0AX0","SIMATIC HMI KP1200 Comfort, Comfort Panel, key operation, 12\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 12 MB configuration memory, Windows CE 6.0, (Microsoft Support included Security updates discontinued) configurable from WinCC Comfort V11",2601,"ST",1,"SIMATIC",5.66,1,"6AV21241MC010AX0"]
["6AV2124-1QC02-0AX1","SIMATIC HMI KP1500 Comfort, Comfort Panel, key operation, 15\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",3563,"ST",1,"SIMATIC",5.76,1,"6AV21241QC020AX1"]
["6AV2124-2DC01-0AX0","SIMATIC HMI KTP400 Comfort, Comfort Panel, Key/touch operation, 4\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 4 MB configuration memory, Windows CE 6.0, (Microsoft Support included Security updates discontinued) configurable from WinCC Comfort V11",679,"ST",1,"SIMATIC",0.68400000000000005,1,"6AV21242DC010AX0"]
["6AV2124-5DC00-0DL0","SIMATIC HMI KTP400 Comfort Comfort Panel, Windows CE 6.0 (Microsoft support including security updates discontinued) Key/touch operation, 4\" widescreen TFT display, with customer-specific design Alfa Laval, Basis: 6AV2124-2DC01-0AX0",759,"ST",1,"SIMATIC",0.68100000000000005,1,"6AV21245DC000DL0"]
["6AV2124-5GC00-0BJ0","SIMATIC HMI TP700 Comfort, Comfort Panel, Touch operation, 7\" widescreen TFT display, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Basic: 6AV2124-0GC01-0AX0",1214,"ST",1,"SIMATIC",1.528,1,"6AV21245GC000BJ0"]
["6AV2124-5GC00-0CJ0","SIMATIC HMI TP700 Comfort, Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with Niehoff design Basic: 6AV2124-0GC01-0AX0",1220,"ST",1,"SIMATIC",1.534,1,"6AV21245GC000CJ0"]
["6AV2124-5GC00-0VS0","SIMATIC HMI TP700 Comfort, Comfort Panel, Touch operation, 7\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 12 MB configuration memory, Windows CE 6.0 (Microsoft Support included Security updates discontinued) configurable from WinCC Comfort V11 with Viessmann design",1220,"ST",1,"SIMATIC",1.532,1,"6AV21245GC000VS0"]
["6AV2124-5GC00-0YY0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific neutral design Basic: 6AV2124-0GC01-0AX0",1220,"ST",1,"SIMATIC",1.5860000000000001,1,"6AV21245GC000YY0"]
["6AV2124-5GC00-2YA0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Basic: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1E-3,1,"6AV21245GC002YA0"]
["6AV2124-5GC00-2YB0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Basic: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1E-3,1,"6AV21245GC002YB0"]
["6AV2124-5GC00-2YC0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Basic: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1E-3,1,"6AV21245GC002YC0"]
["6AV2124-5GC00-2YD0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Basic: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1E-3,1,"6AV21245GC002YD0"]
["6AV2124-5GC00-2YE0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Basic: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1E-3,1,"6AV21245GC002YE0"]
["6AV2124-5GC00-2YF0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Basic: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1E-3,1,"6AV21245GC002YF0"]
["6AV2124-5GC00-2YG0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Basic: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.5,1,"6AV21245GC002YG0"]
["6AV2124-5GC00-2YH0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Basic: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.5,1,"6AV21245GC002YH0"]
["6AV2124-5GC00-2YJ0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Basic: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.5,1,"6AV21245GC002YJ0"]
["6AV2124-5GC00-2YK0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Basic: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.5,1,"6AV21245GC002YK0"]
["6AV2124-5GC00-2YL0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Basic: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.5,1,"6AV21245GC002YL0"]
["6AV2124-5GC00-2YM0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Basic: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.5,1,"6AV21245GC002YM0"]
["6AV2124-5GC00-2YN0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Basic: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.5,1,"6AV21245GC002YN0"]
["6AV2124-5GC00-2YP0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Basic: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.5,1,"6AV21245GC002YP0"]
["6AV2124-5GC00-2YQ0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Basic: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.5,1,"6AV21245GC002YQ0"]
["6AV2124-5GC10-0EH0","SIMATIC HMI TP700 Comfort, Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with METZ design Basic: 6AV2124-0GC01-0AX0 incl. license 6AV2117-0CP00-0BB0",1220,"ST",1,"SIMATIC",1.546,1,"6AV21245GC100EH0"]
["6AV2124-5GC10-0HT0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific design \"HOBART\" Based on: 6AV2124-0GC01-0AX0",1220,"ST",1,"SIMATIC",1.5229999999999999,1,"6AV21245GC100HT0"]
["6AV2124-5GC10-1EH0","SIMATIC HMI TP700 Comfort, with METZ design Bundle, only for Metz",2711,"ST",1,"SIMATIC",5.7,1,"6AV21245GC101EH0"]
["6AV2124-5GC30-0YA0","SIMATIC TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.5620000000000001,1,"6AV21245GC300YA0"]
["6AV2124-5GC30-0YB0","SIMATIC TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.5780000000000001,1,"6AV21245GC300YB0"]
["6AV2124-5GC30-0YD0","SIMATIC TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.5920000000000001,1,"6AV21245GC300YD0"]
["6AV2124-5GC30-0YE0","SIMATIC TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.5669999999999999,1,"6AV21245GC300YE0"]
["6AV2124-5GC30-0YF0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.5640000000000001,1,"6AV21245GC300YF0"]
["6AV2124-5GC30-0YG0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.575,1,"6AV21245GC300YG0"]
["6AV2124-5GC30-0YH0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.6020000000000001,1,"6AV21245GC300YH0"]
["6AV2124-5GC30-0YJ0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.5680000000000001,1,"6AV21245GC300YJ0"]
["6AV2124-5GC30-0YK0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.577,1,"6AV21245GC300YK0"]
["6AV2124-5GC30-0YL0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.5860000000000001,1,"6AV21245GC300YL0"]
["6AV2124-5GC30-0YM0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.5529999999999999,1,"6AV21245GC300YM0"]
["6AV2124-5GC30-0YN0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.5780000000000001,1,"6AV21245GC300YN0"]
["6AV2124-5GC30-0YP0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.55,1,"6AV21245GC300YP0"]
["6AV2124-5GC30-0YQ0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.5649999999999999,1,"6AV21245GC300YQ0"]
["6AV2124-5GC30-0YR0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.56,1,"6AV21245GC300YR0"]
["6AV2124-5GC30-0YS0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.58,1,"6AV21245GC300YS0"]
["6AV2124-5GC30-0YT0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.5920000000000001,1,"6AV21245GC300YT0"]
["6AV2124-5GC30-0YU0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.5860000000000001,1,"6AV21245GC300YU0"]
["6AV2124-5GC30-0YV0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1330,"ST",1,"SIMATIC",1.5740000000000001,1,"6AV21245GC300YV0"]
["6AV2124-5GC30-0YW0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.613,1,"6AV21245GC300YW0"]
["6AV2124-5GC30-0YX0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.5680000000000001,1,"6AV21245GC300YX0"]
["6AV2124-5GC30-1YA0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.605,1,"6AV21245GC301YA0"]
["6AV2124-5GC30-1YC0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.56,1,"6AV21245GC301YC0"]
["6AV2124-5GC30-1YD0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1314,"ST",1,"SIMATIC",1.5680000000000001,1,"6AV21245GC301YD0"]
["6AV2124-5GC30-1YE0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.6,1,"6AV21245GC301YE0"]
["6AV2124-5GC30-1YF0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1E-3,1,"6AV21245GC301YF0"]
["6AV2124-5GC30-1YG0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1E-3,1,"6AV21245GC301YG0"]
["6AV2124-5GC30-1YH0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1430,"ST",1,"SIMATIC",1.61,1,"6AV21245GC301YH0"]
["6AV2124-5GC30-1YJ0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1E-3,1,"6AV21245GC301YJ0"]
["6AV2124-5GC30-1YK0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.56,1,"6AV21245GC301YK0"]
["6AV2124-5GC30-1YL0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.56,1,"6AV21245GC301YL0"]
["6AV2124-5GC30-1YM0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.56,1,"6AV21245GC301YM0"]
["6AV2124-5GC30-1YN0","SIMATIC HMI TP700 Comfort Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Touch operation, 7\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-0GC01-0AX0",1272,"ST",1,"SIMATIC",1.56,1,"6AV21245GC301YN0"]
["6AV2124-5QC00-0YA1","SIMATIC HMI TP1500 Comfort Panel, 15\" widescreen TFT display, with customer-specific Express design Basic: 6AV2124-0QC02-0AX1",3444,"ST",1,"SIMATIC",7.14,1,"6AV21245QC000YA1"]
["6AV2124-5QC00-0YB1","SIMATIC HMI TP1500 Comfort Panel, 15\" widescreen TFT display, with customer-specific Express design Basic: 6AV2124-0QC02-0AX1",3444,"ST",1,"SIMATIC",1E-3,1,"6AV21245QC000YB1"]
["6AV2124-5QC00-0YC1","SIMATIC HMI TP1500 Comfort Panel, 15\" widescreen TFT display, with customer-specific Express design Basic: 6AV2124-0QC02-0AX1",3444,"ST",1,"SIMATIC",7.14,1,"6AV21245QC000YC1"]
["6AV2124-5QC00-0YD1","SIMATIC HMI TP1500 Comfort Panel, 15\" widescreen TFT display, with customer-specific Express design Basic: 6AV2124-0QC02-0AX1",3444,"ST",1,"SIMATIC",7.14,1,"6AV21245QC000YD1"]
["6AV2124-5QC00-0YE1","SIMATIC HMI TP1500 Comfort Panel, 15\" widescreen TFT display, with customer-specific Express design Basic: 6AV2124-0QC02-0AX1",3444,"ST",1,"SIMATIC",7.14,1,"6AV21245QC000YE1"]
["6AV2124-5QC00-0YF1","SIMATIC HMI TP1500 Comfort Panel, 15\" widescreen TFT display, with customer-specific Express design Basic: 6AV2124-0QC02-0AX1",3444,"ST",1,"SIMATIC",7.14,1,"6AV21245QC000YF1"]
["6AV2124-5QC00-0YG1","SIMATIC HMI TP1500 Comfort Panel, 15\" widescreen TFT display, with customer-specific Express design Basic: 6AV2124-0QC02-0AX1",3444,"ST",1,"SIMATIC",7.14,1,"6AV21245QC000YG1"]
["6AV2124-5QC00-0YH1","SIMATIC HMI TP1500 Comfort Panel, 15\" widescreen TFT display, with customer-specific Express design Basic: 6AV2124-0QC02-0AX1",3444,"ST",1,"SIMATIC",7.14,1,"6AV21245QC000YH1"]
["6AV2124-5QC00-0YJ1","SIMATIC HMI TP1500 Comfort Panel, 15\" widescreen TFT display, with customer-specific Express design Basic: 6AV2124-0QC02-0AX1",3444,"ST",1,"SIMATIC",7.14,1,"6AV21245QC000YJ1"]
["6AV2124-5QC00-0YK1","SIMATIC HMI TP1500 Comfort Panel, 15\" widescreen TFT display, with customer-specific Express design Basic: 6AV2124-0QC02-0AX1",3444,"ST",1,"SIMATIC",1.5,1,"6AV21245QC000YK1"]
["6AV2124-5QC00-0YL1","SIMATIC HMI TP1500 Comfort Comfort Panel, 15\" widescreen-TFT display, with customized express design modification based on: 6AV2124-0QC02-0AX1",3444,"ST",1,"SIMATIC",7.14,1,"6AV21245QC000YL1"]
["6AV2124-5QC00-0YM1","SIMATIC HMI TP1500 Comfort Comfort Panel, 15\" widescreen-TFT display, with customized express design modification based on: 6AV2124-0QC02-0AX1",3444,"ST",1,"SIMATIC",7.14,1,"6AV21245QC000YM1"]
["6AV2124-5QC00-0YN1","SIMATIC HMI TP1500 Comfort Comfort Panel, 15\" widescreen-TFT display, with customized express design modification based on: 6AV2124-0QC02-0AX1",3444,"ST",1,"SIMATIC",7.14,1,"6AV21245QC000YN1"]
["6AV2124-5QC00-0YP1","SIMATIC HMI TP1500 Comfort Comfort Panel, 15\" widescreen-TFT display, with customized express design modification based on: 6AV2124-0QC02-0AX1",3444,"ST",1,"SIMATIC",7.14,1,"6AV21245QC000YP1"]
["6AV2124-5QC00-0YQ1","SIMATIC HMI TP1500 Comfort Comfort Panel, 15\" widescreen-TFT display, with customized express design modification based on: 6AV2124-0QC02-0AX1",3444,"ST",1,"SIMATIC",7.14,1,"6AV21245QC000YQ1"]
["6AV2124-5QC00-0YR1","SIMATIC HMI TP1500 Comfort Comfort Panel, 15\" widescreen-TFT display, with customized express design modification based on: 6AV2124-0QC02-0AX1",3444,"ST",1,"SIMATIC",7.14,1,"6AV21245QC000YR1"]
["6AV2124-5QC00-0YS1","SIMATIC HMI TP1500 Comfort Comfort Panel, 15\" widescreen-TFT display, with customized express design modification based on: 6AV2124-0QC02-0AX1",3444,"ST",1,"SIMATIC",7.14,1,"6AV21245QC000YS1"]
["6AV2124-5QC00-0YT1","SIMATIC HMI TP1500 Comfort Comfort Panel, 15\" widescreen-TFT display, with customized express design modification based on: 6AV2124-0QC02-0AX1",3444,"ST",1,"SIMATIC",7.14,1,"6AV21245QC000YT1"]
["6AV2124-5QC00-0YU1","SIMATIC HMI TP1500 Comfort Comfort Panel, 15\" widescreen-TFT display, with customized express design modification based on: 6AV2124-0QC02-0AX1",3444,"ST",1,"SIMATIC",7.14,1,"6AV21245QC000YU1"]
["6AV2124-5QC00-0YV1","SIMATIC HMI TP1500 Comfort Comfort Panel, 15\" widescreen-TFT display, with customized express design modification based on: 6AV2124-0QC02-0AX1",3444,"ST",1,"SIMATIC",7.14,1,"6AV21245QC000YV1"]
["6AV2124-5QC00-0YW1","SIMATIC HMI TP1500 Comfort Comfort Panel, 15\" widescreen TFT display, with customer-specific express design Basis: 6AV2124-0QC02-0AX1",3444,"ST",1,"SIMATIC",7.14,1,"6AV21245QC000YW1"]
["6AV2124-5QC00-0YX1","SIMATIC HMI TP1500 Comfort Comfort Panel, 15\" widescreen TFT display, with customer-specific express design Basis: 6AV2124-0QC02-0AX1",3444,"ST",1,"SIMATIC",7.14,1,"6AV21245QC000YX1"]
["6AV2124-5QC00-1YA1","SIMATIC HMI TP1500 Comfort Comfort Panel, 15\" widescreen TFT display, with customer-specific express design Basis: 6AV2124-0QC02-0AX1",3444,"ST",1,"SIMATIC",7.14,1,"6AV21245QC001YA1"]
["6AV2124-5QC00-1YB1","SIMATIC HMI TP1500 Comfort Comfort Panel, 15\" widescreen TFT display, with customer-specific express design Basis: 6AV2124-0QC02-0AX1",3444,"ST",1,"SIMATIC",7.14,1,"6AV21245QC001YB1"]
["6AV2124-5QC00-1YC1","SIMATIC HMI TP1500 Comfort Comfort Panel, 15\" widescreen TFT display, with customer-specific express design Basis: 6AV2124-0QC02-0AX1",3444,"ST",1,"SIMATIC",7.14,1,"6AV21245QC001YC1"]
["6AV2124-5QC10-1CJ0","Bundle TP1500 NIEHOFF Consisting of: 6AV2124-5QC10-0CJ0, 6AV2181-8XP00-0AX0",3152,"ST",1,"SIMATIC",7.2,1,"6AV21245QC101CJ0"]
["6AV2124-5QC10-2CJ0","Bundle TP1500 Red. Niehoff cnsisting of: 6AV2124-0QC02-0AX1-Z A01+N01, 6AV2181-8XP00-0AX0",3304,"ST",1,"SIMATIC",7.2,1,"6AV21245QC102CJ0"]
["6AV2124-5UC00-0YA1","SIMATIC HMI TP1900 Comfort Comfort Panel, 19\" widescreen-TFT display, with customized express design modification based on: 6AV2124-0UC02-0AX1",4165,"ST",1,"SIMATIC",8.66,1,"6AV21245UC000YA1"]
["6AV2124-5UC00-0YB1","SIMATIC HMI TP1900 Comfort Comfort Panel, 19\" widescreen-TFT display, with customized express design modification based on: 6AV2124-0UC02-0AX1",4165,"ST",1,"SIMATIC",8.66,1,"6AV21245UC000YB1"]
["6AV2124-5UC00-0YC1","SIMATIC HMI TP1900 Comfort Comfort Panel, 19\" widescreen-TFT display, with customized express design modification based on: 6AV2124-0UC02-0AX1",4165,"ST",1,"SIMATIC",8.66,1,"6AV21245UC000YC1"]
["6AV2124-5UC00-0YD1","SIMATIC HMI TP1900 Comfort Comfort Panel, 19\" widescreen-TFT display, with customized express design modification based on: 6AV2124-0UC02-0AX1",4165,"ST",1,"SIMATIC",8.66,1,"6AV21245UC000YD1"]
["6AV2124-5UC00-0YE1","SIMATIC HMI TP1900 Comfort Comfort Panel, 19\" widescreen-TFT display, with customized express design modification based on: 6AV2124-0UC02-0AX1",4165,"ST",1,"SIMATIC",8.66,1,"6AV21245UC000YE1"]
["6AV2124-5UC00-0YF1","SIMATIC HMI TP1900 Comfort Comfort Panel, 19\" widescreen-TFT display, with customized express design modification based on: 6AV2124-0UC02-0AX1",4165,"ST",1,"SIMATIC",8.66,1,"6AV21245UC000YF1"]
["6AV2124-5UC00-0YG1","SIMATIC HMI TP1900 Comfort Comfort Panel, 19\" widescreen-TFT display, with customized express design modification based on: 6AV2124-0UC02-0AX1",4165,"ST",1,"SIMATIC",8.66,1,"6AV21245UC000YG1"]
["6AV2124-5XC00-0YA1","SIMATIC HMI TP2200 Comfort Comfort Panel, 22\" widescreen-TFT display, with customized express design modification based on: 6AV2124-0XC02-0AX1",4875,"ST",1,"SIMATIC",9.2799999999999994,1,"6AV21245XC000YA1"]
["6AV2124-5XC00-0YB1","SIMATIC HMI TP2200 Comfort Comfort Panel, 22\" widescreen-TFT display, with customized express design modification based on: 6AV2124-0XC02-0AX1",4875,"ST",1,"SIMATIC",9.2799999999999994,1,"6AV21245XC000YB1"]
["6AV2124-5XC00-0YC1","SIMATIC HMI TP2200 Comfort Comfort Panel, 22\" widescreen-TFT display, with customized express design modification based on: 6AV2124-0XC02-0AX1",4875,"ST",1,"SIMATIC",9.2799999999999994,1,"6AV21245XC000YC1"]
["6AV2124-5XC00-0YD1","SIMATIC HMI TP2200 Comfort Comfort Panel, 22\" widescreen-TFT display, with customized express design modification based on: 6AV2124-0XC02-0AX1",4875,"ST",1,"SIMATIC",9.2799999999999994,1,"6AV21245XC000YD1"]
["6AV2124-5XC00-0YE1","SIMATIC HMI TP2200 Comfort Comfort Panel, 22\" widescreen-TFT display, with customized express design modification based on: 6AV2124-0XC02-0AX1",4875,"ST",1,"SIMATIC",9.2799999999999994,1,"6AV21245XC000YE1"]
["6AV2124-6DJ00-0AX0","Protective film 4\" widescreen f. KTP400 Basic 1st Generation, KTP400 Basic 2nd Generation, KTP400 Comfort, here the film must be cut. Alternatively: 6AV6574-1AD04-4AA0 Quantity: see technical data",64.099999999999994,"PAK",1,"SIMATIC",0.154,1,"6AV21246DJ000AX0"]
["6AV2124-6GJ00-0AX0","Protective film 7\" widescreen Protective film 7\" widescreen KTP700 Basic 2nd Generation, TP700 Comfort, Further information, Quantity and content: see technical data",86.1,"PAK",1,"SIMATIC",0.19800000000000001,1,"6AV21246GJ000AX0"]
["6AV2124-6JJ00-0AX0","Protective film 9\" widescreen Type 1 for TP900 Comfort, IPC277D Quantity: see technical data",108,"PAK",1,"SIMATIC",0.24299999999999999,1,"6AV21246JJ000AX0"]
["6AV2124-6MJ00-0AX0","protective film 12\" widescreen Type 1 for TP1200 Comfort, IPC277D Quantity: see technical data",129,"PAK",1,"SIMATIC",0.32900000000000001,1,"6AV21246MJ000AX0"]
["6AV2124-6QJ00-0AX1","Protective film 15\" widescreen for Comfort Panel, IPC, Flat Panel, thin client Quantity: see technical data",137,"PAK",1,"SIMATIC",0.40500000000000003,1,"6AV21246QJ000AX1"]
["6AV2124-6UJ00-0AX1","Protective film 19\" widescreen for Comfort Panel, IPC, Flat Panel, thin client Quantity: see technical data",221,"PAK",1,"SIMATIC",0.57999999999999996,1,"6AV21246UJ000AX1"]
["6AV2124-6XJ00-0AX1","Protective film 22\" widescreen for Comfort Panel, IPC, Flat Panel, thin client Quantity: see technical data",231,"PAK",1,"SIMATIC",0.72299999999999998,1,"6AV21246XJ000AX1"]
["6AV2124-7DC31-0YA0","SIMATIC HMI KTP400 Comfort, Comfort Panel, Windows CE 6.0 (Microsoft Support included Security updates discontinued) Key/touch operation, without LED, 4\" widescreen TFT display, with customer-specific Express design Based on: 6AV2124-2DC01-0AX0",824,"ST",1,"SIMATIC",0.66800000000000004,1,"6AV21247DC310YA0"]
["6AV2125-2AE03-0AX0","SIMATIC HMI connection box compact for Mobile Panels, installation in control cabinet, PROFINET and PROFIsafe, connection of safety relay, Connection point detection",150,"ST",1,"SIMATIC",0.47499999999999998,1,"6AV21252AE030AX0"]
["6AV2125-2AE13-0AX0","SIMATIC HMI connection box Standard for Mobile Panels, wall mounting, PROFINET and PROFIsafe, connection of safety relay, terminal detection, integrated switch",311,"ST",1,"SIMATIC",0.77800000000000002,1,"6AV21252AE130AX0"]
["6AV2125-2AE23-0AX0","SIMATIC HMI connection box Advanced for Mobile Panels, wall mounting, PROFINET and PROFIsafe, connection of safety relay, emergency stop circuit bridging, terminal detection, Integrated switch, MRP client, IRT",418,"ST",1,"SIMATIC",0.78,1,"6AV21252AE230AX0"]
["6AV2125-2DB23-0AX0","SIMATIC HMI KTP400F Mobile with integrated acknowledgement button, emergency switching-off switch, Touch and Key operation, 4\" widescreen TFT display, PROFINET interface, configurable from WinCC Comfort V13 SP1 with HSP",1040,"ST",1,"SIMATIC",0.88200000000000001,1,"6AV21252DB230AX0"]
["6AV2125-2GB03-0AX0","SIMATIC HMI KTP700 Mobile, 7.0\" TFT display, 800x 480 pixel, 16m colors, key and touch operation, 8 function keys, 1x PROFINET/Industrial Ethernet interface, 1x multimedia card, 1x USB, configurable from WinCC Comfort V13 SP1",1982,"ST",1,"SIMATIC",1.2589999999999999,1,"6AV21252GB030AX0"]
["6AV2125-2GB23-0AX0","SIMATIC HMI KTP700F Mobile, 7.0\" TFT display, 800x 480 pixel, 16m colors, key and touch operation, 8 function keys, 1x PROFINET/Industrial Ethernet interface, 1x multimedia card, 1x USB, Key-operated switch, acknowledgement button, 1 emergency stop/stop button configurable from WinCC Comfort V13 SP1",2303,"ST",1,"SIMATIC",1.383,1,"6AV21252GB230AX0"]
["6AV2125-2JB03-0AX0","SIMATIC HMI KTP900 Mobile, 9.0\" TFT display, 800x 480 pixel, 16 million colors. key and touch operation, 10 function keys, 1x PROFINET/Industrial Ethernet interface, 1x multimedia card, 1x USB, configurable from WinCC Comfort V13 SP1",3053,"ST",1,"SIMATIC",1.635,1,"6AV21252JB030AX0"]
["6AV2125-2JB23-0AX0","SIMATIC HMI KTP900F Mobile, 9.0\" TFT display, 800x 480 pixel, 16m colors, key and touch operation, 10 function keys, 1x PROFINET/Industrial Ethernet interface, 1x multimedia card, 1x USB, Key-operated switch, acknowledgement button, 1 emergency stop/stop button configurable from WinCC Comfort V13 SP1",3374,"ST",1,"SIMATIC",1.736,1,"6AV21252JB230AX0"]
["6AV2132-0HA00-0AA1","LOGO!+KP300 Basic Starter Kit LOGO! 12/24RCE, HMI KP300 Basic mono PN, LOGO! Power 24 V 1.3 A, LOGO! SOFT Comfort V8, WinCC Basic, information material, in SYSTAINER",489,"ST",1,"SIMATIC",3,1,"6AV21320HA000AA1"]
["6AV2132-0KA00-0AA1","LOGO!+KTP400 Basic Starter Kit LOGO! 12/24RCE, HMI KTP400 Basic, LOGO! Power 24 V 1.3 A, LOGO! SOFT Comfort V8, WinCC Basic, information material, in SYSTAINER",652,"ST",1,"SIMATIC",3,1,"6AV21320KA000AA1"]
["6AV2132-3GB00-0AA1","LOGO!+KTP700 Basic Starter Kit LOGO! 12/24RCE, HMI KTP700 Basic, LOGO! Power 24 V 1.3 A, LOGO! SOFT Comfort V8, WinCC Basic, information material, in SYSTAINER",1142,"ST",1,"SIMATIC",3.5,1,"6AV21323GB000AA1"]
["6AV2133-4AF00-0AA0","Trainer Package TP700 Comfort Consisting of: TP700 Comfort, 6 m cross cable, WinCC Advanced for Panels, SW and documentation on DVD, License on USB stick for WinCC Advanced Engineering, Runtime, Options for educational purposes only",812,"ST",1,"SIMATIC",2.5,1,"6AV21334AF000AA0"]
["6AV2133-4BF00-0AA0","Trainer Package TP1500 Comfort Consisting of: TP1500 Comfort, 6 m cross cable, WinCC Advanced for Panels, SW and documentation on DVD, License on USB stick for WinCC Advanced Engineering, Runtime, Options for educational purposes only",1792,"ST",1,"SIMATIC",7.8,1,"6AV21334BF000AA0"]
["6AV2133-5GA00-0AA0","Starter kit Mobile Panel Consisting of: 1x KTP700F Mobile, 1x connection box Standard, 1x connecting cable 2 m, 1x wall holder, 1x WinCC Comfort (TIA Portal)",2839,"ST",1,"SIMATIC",4.7050000000000001,1,"6AV21335GA000AA0"]
["6AV2143-6GB00-0AA0","SIMATIC HMI, TP700 Basic, Basic Panel, Neutral design, Touch operation, 7\" TFT display, 65536 colors, PROFINET interface, configurable from WinCC Basic V13/ STEP 7 Basic V13, contains open-source software, which is provided free of charge see enclosed CD",656,"ST",1,"SIMATIC",0.97699999999999998,1,"6AV21436GB000AA0"]
["6AV2143-8GB50-0AA0","SIMATIC HMI, IWP700, Industrial Webpanel, Key/touch operation, 7\" TFT display, 65536 colors, PROFINET interface, HTML5, stand-alone, WinCC configuration not necessary, contains open-source software, which is provided free of charge",643,"ST",1,"SIMATIC",0.97699999999999998,1,"6AV21438GB500AA0"]
["6AV2143-8JB50-0AA0","SIMATIC HMI, IWP900, Industrial Webpanel, Key/touch operation, 9\" TFT display, 65536 colors, PROFINET interface, HTML5, stand-alone, WinCC configuration not necessary, contains open-source software, which is provided free of charge",1125,"ST",1,"SIMATIC",1.1299999999999999,1,"6AV21438JB500AA0"]
["6AV2143-8MB50-0AA0","SIMATIC HMI, IWP1200, Industrial Webpanel, Key/touch operation, 12\" TFT display, 65536 colors, PROFINET interface, HTML5, stand-alone, WinCC configuration not necessary, contains open-source software, which is provided free of charge",1607,"ST",1,"SIMATIC",2.1619999999999999,1,"6AV21438MB500AA0"]
["6AV2144-6GC00-1AA0","SIMATIC HMI TP700 Comfort, Base, touch operation, 7\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB user memory, Windows CE 6.0, configurable from WinCC Comfort V11 SP2",1082,"ST",1,"SIMATIC",1.5609999999999999,1,"6AV21446GC001AA0"]
["6AV2144-6MC00-1AA0","SIMATIC HMI TP1200 Comfort, Base, touch operation, 12\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB user memory, Windows CE 6.0, configurable from WinCC Comfort V11 SP2",1806,"ST",1,"SIMATIC",3.7,1,"6AV21446MC001AA0"]
["6AV2144-8GC10-0AA0","SIMATIC HMI TP700 Comfort INOX, Stainless steel front, Con- tinuous decorative film, Degree of protection front IP66K, 7\" widescreen TFT display, PROFINET interface, MPI/PROFIBUS DP interface, 12 MB configuration memory, Windows CE 6.0, (Microsoft Support included Security updates discontinued) configurable from WinCC Comfort V11",1512,"ST",1,"SIMATIC",2.157,1,"6AV21448GC100AA0"]
["6AV2144-8JC10-0AA0","SIMATIC HMI TP900 Comfort INOX Stainless steel front, Continuous decorative film, Degree of protection front IP66K, 9\" widescreen TFT display, PROFINET interface, MPI/PROFIBUS DP interface, 12 MB configuration memory, Windows CE 6.0, (Microsoft Support included Security updates discontinued) configurable from WinCC Comfort V11",2205,"ST",1,"SIMATIC",2.9,1,"6AV21448JC100AA0"]
["6AV2144-8JC20-0AA0","SIMATIC HMI TP900 Comfort INOX Stainless steel front, Glass pane, capacitive touch, Degree of protection front IP69K, 9\" widescreen TFT display, PROFINET interface, MPI/PROFIBUS DP interface, 12 MB configuration memory, Windows CE 6.0, (Microsoft Support included Security updates discontinued) configurable from WinCC Comfort V15",2518,"ST",1,"SIMATIC",1E-3,1,"6AV21448JC200AA0"]
["6AV2144-8MC10-0AA0","SIMATIC HMI TP1200 Comfort INOX Stainless steel front, Con- tinuous decorative film, Degree of protection front IP66K, 12\" widescreen TFT display, PROFINET interface, MPI/PROFIBUS DP interface, 12 MB configuration memory, Windows CE 6.0, (Microsoft Support included Security updates discontinued) configurable from WinCC Comfort V11",2772,"ST",1,"SIMATIC",4.359,1,"6AV21448MC100AA0"]
["6AV2144-8MC20-0AA0","SIMATIC HMI TP1200 Comfort INOX Stainless steel front, Glass pane, capacitive touch, Degree of protection front IP69K, 12\" widescreen TFT display, PROFINET interface, MPI/PROFIBUS DP interface, 12 MB configuration memory, Windows CE 6.0, (Microsoft Support included Security updates discontinued) configurable from WinCC Comfort V15",2730,"ST",1,"SIMATIC",1E-3,1,"6AV21448MC200AA0"]
["6AV2144-8QC10-0AA0","SIMATIC HMI TP1500 Comfort INOX Stainless steel front, Con- Continuous decorative film, Degree of protection front IP66K, 15\" widescreen TFT display, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, Windows CE 6.0, (Microsoft Support included Security updates discontinued) configurable from WinCC Comfort V11 SP2",3654,"ST",1,"SIMATIC",9.3000000000000007,1,"6AV21448QC100AA0"]
["6AV2144-8UC10-0AA0","SIMATIC HMI TP1900 Comfort INOX Stainless steel front, Con- Continuous decorative film, Degree of protection front IP66K, 19\" widescreen TFT display, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, Windows CE 6.0, (Microsoft Support included Security updates discontinued) configurable from WinCC Comfort V11 SP2",4158,"ST",1,"SIMATIC",1E-3,1,"6AV21448UC100AA0"]
["6AV2145-8GB00-0AA0","SIMATIC HMI KTP700F Mobile HW, 7.0\" TFT display, 800 x 480 pixel,16m colors key and touch operation, 6 function keys, 2 illuminated push-buttons, 1x PROFINET/Industrial Ethernet interface, 1x multimedia card, 1x USB, Key-operated switch, acknowledgement switch, emergency stop/stop button configurable from WinCC Comfort V15, handwheel",2583,"ST",1,"SIMATIC",1E-3,1,"6AV21458GB000AA0"]
["6AV2145-8GB01-0AA0","SIMATIC HMI KTP700F Mobile HW/OR, 7.0\" TFT display, 800 x 480 pixel,16m colors key and touch operation, 6 function keys, 2 illuminated push-buttons, 1x PROFINET/Industrial Ethernet interface, 1x multimedia card, 1x USB, Key-operated switch, acknowledgement switch, emergency stop/stop button configurable from WinCC Comfort V15, handwheel and override",2783,"ST",1,"SIMATIC",1E-3,1,"6AV21458GB010AA0"]
["6AV2153-0XX05-0AH5","SIMATIC WinCC Unified Engineering V15.1; delivery only after special sales release; engineering software; Floating License; Software, documentation and license key for download ******************************* e-mail address required for delivery",525,"ST",1,"SIMATIC",1E-3,1,"6AV21530XX050AH5"]
["6AV2155-0XX05-0AH0","SIMATIC WinCC Unified Runtime V15.1; delivery only after special sales release; runtime software; runtime license; Software, documentation and license key for download ******************************* e-mail address required for delivery",525,"ST",1,"SIMATIC",1E-3,1,"6AV21550XX050AH0"]
["6AV2156-0BC01-5LH0","SIMATIC WinCC Unified Calendar V15.1; delivery only after special sales release; engineering/runtime software; single license; software, documentation and license certificate for download ******************************* e-mail address required for delivery",158,"ST",1,"SIMATIC",1E-3,1,"6AV21560BC015LH0"]
["6AV2156-0BL01-5LH0","SIMATIC WinCC Unified Line Coordination V15.1; delivery only after special sales release; engineering/runtime software; single license; software, documentation and license certificate for download ******************************* e-mail address required for delivery",158,"ST",1,"SIMATIC",1E-3,1,"6AV21560BL015LH0"]
["6AV2156-0BP01-5LH0","SIMATIC WinCC Unified Performance Insight V15.1; delivery only after special sales release; engineering/runtime software; single license; software, documentation and license certificate for download ******************************* e-mail address required for delivery",158,"ST",1,"SIMATIC",1E-3,1,"6AV21560BP015LH0"]
["6AV2156-0BS01-5LH0","SIMATIC WinCC Unified Sequence Execution V15.1; delivery only after special sales release; engineering/runtime software; single license; software, documentation and license certificate for download ******************************* e-mail address required for delivery",158,"ST",1,"SIMATIC",1E-3,1,"6AV21560BS015LH0"]
["6AV2158-0XX00-0XY0","SIMATIC WinCC Unified SUS (download) for pilot customers ******************************* Requirement: signed pilot customer agreement ******************************* E-mail address required for delivery",5.3,"ST",1,"SIMATIC",1E-3,1,"6AV21580XX000XY0"]
["6AV2170-0AA10-0AA0","SIMATIC Notifier Server 1.0 for Win7 or Win10 (64 Bit), Together with the SIMATIC Notifier app (for Smartwatches with Android Wear2, available through Google Play) it enables sending configur. notifications to specific users via WIFI. The connection to the plant or machine is realised via S7 or OPC UA connection. ^User & Role Management, *Diff. notification categories, *Takeover function for teams, *Unicode text for messages, *Unlimited Server License (ALM)*-Incl.1 Client Lic. extendable ************************* E-Mail address required for delivery",490,"ST",1,"SIMATIC",1E-3,1,"6AV21700AA100AA0"]
["6AV2170-0AA20-0AA0","SIMATIC Notifier Client License for SIMATIC Notifier Server (6AV2170-0AA10-0AA0). SIMATIC Notifier Server already includes one Client License, which allows to connect 1x smart device to the Notifier Server. If you need more than 1x device connected, this license enables you to add several additional clients to the SIMATIC Notifier system. *Type: Floating ALM license, *freely extendable, *Smartwatch, -phone or tablet ************************* E-Mail address required for delivery",164,"ST",1,"SIMATIC",1E-3,1,"6AV21700AA200AA0"]
["6AV2181-3JJ20-0AX0","Protective film 9\" widescreen, Type 2 for KTP900 Basic Quantity: see technical data",108,"PAK",1,"SIMATIC",0.23799999999999999,1,"6AV21813JJ200AX0"]
["6AV2181-3MJ20-0AX0","protective film 12\" widescreen Type 2 for KTP1200 Basic Quantity: see technical data",174,"PAK",1,"SIMATIC",0.35699999999999998,1,"6AV21813MJ200AX0"]
["6AV2181-4DM10-0AX0","Memory card interlock Plastic for Comfort panel 4β€\u009d, Backs up memory card from falling out Further information, Quantity and content: see technical data",42,"PAK",1,"SIMATIC",1.9E-2,1,"6AV21814DM100AX0"]
["6AV2181-4XM00-0AX0","Memory card interlock Comfort panel 7 ... 22\", Plastic for Backs up memory card from falling out Further information, Quantity and content: see technical data",42,"PAK",1,"SIMATIC",3.5999999999999997E-2,1,"6AV21814XM000AX0"]
["6AV2181-5AF02-0AX0","SIMATIC HMI connecting cable for KTPX00(F) Mobile, Length 2 m",126,"ST",1,"SIMATIC",0.311,1,"6AV21815AF020AX0"]
["6AV2181-5AF05-0AX0","SIMATIC HMI connecting cable for KTPX00(F) Mobile, length 5 m",158,"ST",1,"SIMATIC",0.57999999999999996,1,"6AV21815AF050AX0"]
["6AV2181-5AF08-0AX0","SIMATIC HMI connecting cable for KTPX00(F) Mobile, Length 8 m",189,"ST",1,"SIMATIC",0.93100000000000005,1,"6AV21815AF080AX0"]
["6AV2181-5AF10-0AX0","SIMATIC HMI connecting cable for KTPX00(F) Mobile, length 10 m",210,"ST",1,"SIMATIC",1.044,1,"6AV21815AF100AX0"]
["6AV2181-5AF15-0AX0","SIMATIC HMI connecting cable for KTPX00(F) Mobile, Length 15 m",252,"ST",1,"SIMATIC",1.5880000000000001,1,"6AV21815AF150AX0"]
["6AV2181-5AF20-0AX0","SIMATIC HMI connecting cable for KTPX00(F) Mobile, Length 20 m",294,"ST",1,"SIMATIC",2.1549999999999998,1,"6AV21815AF200AX0"]
["6AV2181-5AF25-0AX0","SIMATIC HMI connecting cable for KTPX00(F) Mobile, Length 25 m",315,"ST",1,"SIMATIC",2.6190000000000002,1,"6AV21815AF250AX0"]
["6AV2181-5AG80-0AX0","Wall holder, Type 13 for KTP400F mobile, KTP700 Mobile KTP700F Mobile, KTP900 Mobile, KTP900F Mobile, without attachment parts, incl. cable tray Further information, Quantity and content: see technical data",104,"ST",1,"SIMATIC",1.1639999999999999,1,"6AV21815AG800AX0"]
["6AV2181-5AL10-0AX0","Power supply unit, external, for Mobile Panel IWLAN DE incl. power supply cable for Germany, France, Spain Netherlands, Belgium Sweden Austria Finland Further information, Quantity and content: see technical data",116,"ST",1,"SIMATIC",0.56000000000000005,1,"6AV21815AL100AX0"]
["6AV2181-5AL20-0AX0","Power supply unit, external, for Mobile Panel IWLAN UK, incl. power supply cable for United Kingdom Further information, Quantity and content: see technical data",116,"ST",1,"SIMATIC",0.56000000000000005,1,"6AV21815AL200AX0"]
["6AV2181-5AL30-0AX0","Power supply unit, external, for Mobile Panel IWLAN SW, incl. power supply cable for Switzerland Further information, Quantity and content: see technical data",116,"ST",1,"SIMATIC",0.53,1,"6AV21815AL300AX0"]
["6AV2181-5AL40-0AX0","Power supply unit, external, for Mobile Panel IWLAN US, incl. power supply cable for USA Further information, Quantity and content: see technical data",116,"ST",1,"SIMATIC",0.56000000000000005,1,"6AV21815AL400AX0"]
["6AV2181-5AL50-0AX0","Power supply unit, external, for Mobile Panel IWLAN IT, incl. power supply cable for Italy Further information, Quantity and content: see technical data",116,"ST",1,"SIMATIC",0.52,1,"6AV21815AL500AX0"]
["6AV2181-5AL60-0AX0","Power supply unit, external, for Mobile Panel IWLAN CN, incl. power supply cable for China Further information, Quantity and content: see technical data",116,"ST",1,"SIMATIC",0.54,1,"6AV21815AL600AX0"]
["6AV2181-5AR80-0AX0","Spare key type 13 for key-operated switch KTP Mobile Panels 2nd Generation Further information, Quantity and content: see technical data",94.5,"ST",1,"SIMATIC",1.4E-2,1,"6AV21815AR800AX0"]
["6AV2181-5DJ00-0AX0","Protective film 4\" widescreen, type 13 Protective film 4\" widescreen KTP400F Mobile 4\" widescreen Further information, Quantity and content: see technical data",52.5,"ST",1,"SIMATIC",0.13800000000000001,1,"6AV21815DJ000AX0"]
["6AV2181-5DJ10-0AX0","Labeling set 4β€\u009d wide, type 13 Labeling set 4β€\u009d wide KTP400F Mobile 4\" Further information, Quantity and content: see technical data",78.8,"ST",1,"SIMATIC",0.06,1,"6AV21815DJ100AX0"]
["6AV2181-5GJ00-0AX0","Protective film 7\" widescreen, type 13 Protective film 7\" widescreen KTP700 Mobile KTP700F Mobile Further information, Quantity and content: see technical data",94.5,"ST",1,"SIMATIC",0.16600000000000001,1,"6AV21815GJ000AX0"]
["6AV2181-5GJ10-0AX0","Labeling set 7β€\u009d wide, type 13 Labeling set 7β€\u009d wide KTP700 Mobile KTP700F Mobile Further information, Quantity and content: see technical data",84,"ST",1,"SIMATIC",0.08,1,"6AV21815GJ100AX0"]
["6AV2181-5JJ00-0AX0","Protective film 9\" widescreen, type 13 Protective film 9\" widescreen, KTP900 Mobile, KTP900F Mobile Further information, Quantity and content: see technical data",105,"ST",1,"SIMATIC",0.187,1,"6AV21815JJ000AX0"]
["6AV2181-5JJ10-0AX0","Labeling set 9β€\u009d wide, type 13 Labeling set 9β€\u009d wide KTP900 Mobile, KTP900F Mobile Further information, Quantity and content: see technical data",94.5,"ST",1,"SIMATIC",0.1,1,"6AV21815JJ100AX0"]
["6AV2181-8AQ10-0AX0","SIMATIC SD outdoor card 2 GB, Secure Digital Card, For outdoor and indoor use Further information, Quantity and content: see technical data see technical data",78.8,"ST",1,"SIMATIC",0.03,1,"6AV21818AQ100AX0"]
["6AV2181-8AS20-0AX0","SIMATIC HMI USB flash drive, 8 GB, for HMI devices with corresponding Slot Further information, Quantity and content: see technical data",179,"ST",1,"SIMATIC",1.7000000000000001E-2,1,"6AV21818AS200AX0"]
["6AV2181-8AT00-0AX0","USB 2.0 mouse for devices with corresponding interface Further information, Quantity and content: see technical data",52.5,"ST",1,"SIMATIC",0.20799999999999999,1,"6AV21818AT000AX0"]
["6AV2181-8AV20-0AX0","touch pen system for capacitive or resistive touch screen Pen incl. holder for 22.5 mm, screw on or glue for capacitive and resistive touch screens Further information, Quantity and content: see technical data",99.8,"ST",1,"SIMATIC",0.13400000000000001,1,"6AV21818AV200AX0"]
["6AV2181-8AV60-0AX0","Touch pen caps Replacement caps for touch pen system for capacitive and resistive touch screens Further information, Quantity and content: see technical data",26.3,"ST",1,"SIMATIC",0.01,1,"6AV21818AV600AX0"]
["6AV2181-8XA80-0AX0","Service set 6β€\u009d devices, type 2 Service set for TP 070, TP 170A/B, OP 170B, TP 170micro, OP /TP 270 6\", MP 177 6\"T, MP 270B 6\" Touch Further information, Quantity and content: see technical data",108,"ST",1,"SIMATIC",0.77500000000000002,1,"6AV21818XA800AX0"]
["6AV2181-8XP00-0AX0","SIMATIC SD memory card 2 GB Secure Digital Card for For devices with corresponding Slot Further information, Quantity and content: see technical data",78.8,"ST",1,"SIMATIC",0.03,1,"6AV21818XP000AX0"]
["6AV2185-4GA00-0AX0","Service package for TP700 Comfort INOX Consisting of: device seal, clamping frame, mounting clips, connecting terminals, Installation instructions",85.699999999999989,"ST",1,"SIMATIC",0.35799999999999998,1,"6AV21854GA000AX0"]
["6AV2185-4JA00-0AX0","Service package for TP900 Comfort INOX Consisting of: device seal, clamping frame, mounting clips, connecting terminals, Installation instructions",94.3,"ST",1,"SIMATIC",0.5,1,"6AV21854JA000AX0"]
["6AV2185-4JA10-0AX0","Service package for TP900 Comfort INOX PCT Consisting of: Device seal, clamping frame, mounting clips, connection terminals, installation instructions",92.4,"ST",1,"SIMATIC",0.5,1,"6AV21854JA100AX0"]
["6AV2185-4MA00-0AX0","Service package for TP1200 Comfort INOX Consisting of: device seal, clamping frame, mounting clips, connecting terminals, Installation instructions",102,"ST",1,"SIMATIC",0.53700000000000003,1,"6AV21854MA000AX0"]
["6AV2185-4MA01-0AX0","Service package for TP1200 Comfort INOX LF Consisting of: device seal, clamping frame, mounting clips, connecting terminals, Installation instructions",102,"ST",1,"SIMATIC",0.56999999999999995,1,"6AV21854MA010AX0"]
["6AV2185-4QA00-0AX0","Service package for TP1500 Comfort INOX Consisting of: device seal, clamping frame, mounting clips, connecting terminals, Installation instructions",140,"ST",1,"SIMATIC",1.002,1,"6AV21854QA000AX0"]
["6AV2185-4UA00-0AX0","Service package for TP1900 Comfort INOX and ITC 1900 INOX Consisting of: device seal, clamping frame, mounting clips, connecting terminals, Installation instructions",156,"ST",1,"SIMATIC",1.03,1,"6AV21854UA000AX0"]
["6AV2185-8CE01-0AA0","Extension Unit 12\" KP12 PN for mounting on all fully IP65-enclosed 16:9 HMI/IPC devices. For the flexible installation of operator controls, 3 mounting positions, 3 operator controls equippable; Connection via PROFINET (without equipment)",698,"ST",1,"SIMATIC",2.2000000000000002,1,"6AV21858CE010AA0"]
["6AV2185-8CE08-0AA0","Extension Unit 12\" KP24 PN for mounting on all fully IP65-enclosed 16:9 HMI/IPC devices. Without free installation positions. Connection via PROFINET",1254,"ST",1,"SIMATIC",2.2000000000000002,1,"6AV21858CE080AA0"]
["6AV2185-8CF01-0AA0","Extension Unit 12\" KP12F PN compatible with all IP65 fully enclosed 16:9 HMI/IPC devices. Flexible configuration of control elements; 3 mounting positions; 3 control elements can be installed. PROFIsafe connection (control elements ordered separately)",830,"ST",1,"SIMATIC",2.2000000000000002,1,"6AV21858CF010AA0"]
["6AV2185-8CF41-0SW0","Extension Unit 12\" KP12F PN, compatible with all IP65 fully enclosed 16:9 HMI/IPC devices. 1x E-Stop, 1x keyselector (2 positions), connection via PROFIsafe, completely mounted, customized",1124,"ST",1,"SIMATIC",2.2000000000000002,1,"6AV21858CF410SW0"]
["6AV2185-8DE01-0AA0","Extension Unit 15\" KP12 PN for mounting on all fully IP65-enclosed 16:9 HMI/IPC devices. For the flexible installation of operator controls, 5 installation positions 5 operator controls equippable; Connection via PROFINET (without equipment)",803,"ST",1,"SIMATIC",2.5,1,"6AV21858DE010AA0"]
["6AV2185-8DE08-0AA0","Extension Unit 15\" KP36 PN for mounting on all fully IP65-enclosed 16:9 HMI/IPC devices. Without free installation positions. Connection via PROFINET",1426,"ST",1,"SIMATIC",2.5,1,"6AV21858DE080AA0"]
["6AV2185-8DF01-0AA0","Extension Unit 15\" KP12F PN compatible with all IP65 fully enclosed 16:9 HMI/IPC devices. Flexible configuration of control elements; 5 mounting positions; 5 control elements can be installed. PROFIsafe connection (control elements ordered separately)",935,"ST",1,"SIMATIC",2.5,1,"6AV21858DF010AA0"]
["6AV2185-8ED40-0AT0","Extension Unit 19\" PROFIsafe for mounting on all fully IP65-enclosed 16:9 HMI/IPC 1x EMERGENCY OFF 6x illuminated pushbutton 1x key-operated pushbutton 1x selector switch Connection via PROFIsafe BTO Customized",1399,"ST",1,"SIMATIC",2.8,1,"6AV21858ED400AT0"]
["6AV2185-8ED40-0FD0","Extension Unit 19\" PROFIsafe, for mounting on all fully IP65-enclosed 16:9 HMI/IPC 1x EMERGENCY STOPP, 1x illuminated push-button, Connection via PROFIsafe, BTO Customized",1027,"ST",1,"SIMATIC",1E-3,1,"6AV21858ED400FD0"]
["6AV2185-8ED40-0PR0","Extension Unit 19\" PROFIsafe, for mounting on all fully IP65-enclosed 16:9 HMI/IPC, 1x E-Stop, 8x illuminated push button, 1x selector switch, Connection via PROFIsafe Project customized",1412,"ST",1,"SIMATIC",2.8,1,"6AV21858ED400PR0"]
["6AV2185-8EE01-0AA0","Extension unit 19\" KP12 PN for mounting on all fully IP65-protected 16:9 HMI/IPC devices. For the flexible installation of operator controls, 6 mounting positions, 6 operator controls equippable; Connection via PROFINET (without equipment)",876,"ST",1,"SIMATIC",2.7,1,"6AV21858EE010AA0"]
["6AV2185-8EE08-0AA0","Extension Unit 19\" KP36 PN for mounting on all fully IP65-enclosed 16:9 HMI/IPC devices. Without free installation positions. Connection via PROFINET",1500,"ST",1,"SIMATIC",2.7,1,"6AV21858EE080AA0"]
["6AV2185-8EF01-0AA0","Extension unit 19\" KP12F PN for mounting on all fully IP65-protected 16:9 HMI/IPC devices. For the flexible installation of operator controls, 6 mounting positions, 6 operator controls equippable. Connection via PROFIsafe (without equipment)",1008,"ST",1,"SIMATIC",2.7,1,"6AV21858EF010AA0"]
["6AV2185-8EF41-0LP0","Extension unit 19\" KP12 PN, for mounting on all fully IP65-protected 16:9 HMI/IPC, 1x RGB push Button, 1x key switch, 2x illuminated push-button, 1x Emergency Stopping, 1x KP12F PN, Connection via PROFINET",1610,"ST",1,"SIMATIC",1E-3,1,"6AV21858EF410LP0"]
["6AV2185-8EF41-0SW0","Extension Unit 19\" KP12F PN, for mounting on all fully IP65-enclosed 16:9 HMI/IPC devices, 1 Emergency Stop, 1x key-operated switch (2 positions), connection via PROFIsafe, fully assembled Customized: KP12 labeled",1342,"ST",1,"SIMATIC",2.7,1,"6AV21858EF410SW0"]
["6AV2185-8FD40-0EM0","Extension Unit 22\" PROFIsafe for mounting on all fully IP65-enclosed 16:9 HMI/IPC, 1x emergency off, 2x illuminated pushbutton, 1x selector switch, PROFIsafe connection BTO Labeling holder, Customer-specific",1164,"ST",1,"SIMATIC",2.9,1,"6AV21858FD400EM0"]
["6AV2185-8FE01-0AA0","Extension unit 22\" KP12 PN for mounting on all fully IP65-protected 16:9 HMI/IPC devices. For the flexible installation of operator controls, 8 mounting positions, 8 operator controls equippable; Connection via PROFINET (without equipment)",908,"ST",1,"SIMATIC",2.8,1,"6AV21858FE010AA0"]
["6AV2185-8FE08-0AA0","Extension Unit 22\" KP48 PN for mounting on all fully IP65-enclosed 16:9 HMI/IPC devices. Without free installation positions. Connection via PROFINET",1531,"ST",1,"SIMATIC",2.8,1,"6AV21858FE080AA0"]
["6AV2185-8FF01-0AA0","Extension unit 22\" KP12F PN for mounting on all fully IP65-protected 16:9 HMI/IPC devices. For the flexible installation of operator controls, 8 mounting positions, 8 operator controls equippable. Connection via PROFIsafe (without equipment)",1040,"ST",1,"SIMATIC",2.8,1,"6AV21858FF010AA0"]
["6AV2185-8FF41-0DD0","Extension unit 22\" KP12F PN, mounting on all fully IP65-protected 16:9 HMI/IPC devices. 7x RGB-Button, 1x E-Stop, Connection via PROFIsafe, complete mounted, customized",1908,"ST",1,"SIMATIC",2.8,1,"6AV21858FF410DD0"]
["6AV2185-8MA00-0AA0","Aluminum diecast mounting clip with 24 VDC plug for INOX Panels, ITC INOX, FP INOX, IFP INOX, Displays from 7\" to 22\", sheet thickness 1.5...6 mm, Further information, Quantity: see technical data",83.6,"ST",1,"SIMATIC",0.18,1,"6AV21858MA000AA0"]
["6AV3678-3XC30","Service package for PP7, PP17 I, PP17 II, 1x mounting seal PP7, 1x mounting seal PP17, 5x mounting clamps, 1x 24 V DC connector 2-pole, 1x 24 V DC connector 3-pole, 1x connector 4-pole, 2x connectors 16-pole",110,"ST",1,"SIMATIC",0.5,1,"6AV36783XC30"]
["6AV3688-3AF37-0AX0","SIMATIC HMI KP8F PN, Key Panel, 8 short-stroke switches with multi-colored LEDs, PROFINET interfaces with PROFIsafe; 8 DI/DO and 2 safety DI pins, 24 V DC can be looped through parameterizable as of STEP 7 V5.5",431,"ST",1,"SIMATIC",0.35499999999999998,1,"6AV36883AF370AX0"]
["6AV3688-3AY36-0AX0","SIMATIC HMI KP8 PN Key Panel, 8 short-stroke switches with multi-colored LEDs, PROFINET interfaces 8 configurable DI/DO pins, 24 V DC can be looped through parameterizable as of STEP 7 V5.5",298,"ST",1,"SIMATIC",0.32600000000000001,1,"6AV36883AY360AX0"]
["6AV3688-3EH47-0AX0","SIMATIC HMI KP32F PN, Key Panel, 32 short-stroke keys with multi-colored LEDs, PROFINET interfaces with PROFIsafe, 16 DI+16 DI/DO, 4 safety DI pins, 24 V DC can be looped through parameterizable as of STEP 7 V5.5",1214,"ST",1,"SIMATIC",1.907,1,"6AV36883EH470AX0"]
["6AV3688-3XY38-3AX0","design empty front in KP8 format for easy mounting of standard 22.5 mm operator controls Ideal for setting up modular operator panels also suitable for installation in extension units of the pro devices",163,"ST",1,"SIMATIC",0.31,1,"6AV36883XY383AX0"]
["6AV3688-5AY00-0YY0","SIMATIC HMI KP8 PN Key Panel, Neutral front, 8 short-stroke switches with multi-colored LEDs, PROFINET interfaces 8 configurable DI/DO pins, 24 V DC can be looped through parameterizable as of STEP 7 V5.5 Basic: 6AV3688-3AY36-0AX0",341,"ST",1,"SIMATIC",0.316,1,"6AV36885AY000YY0"]
["6AV6333-1GA00-0AX0","SIMATIC WinCC Add-ons Design consisting of WinCC Connectivity Pack, WinCC/ODK, WinCC/Industrialx",3602,"ST",1,"SIMATIC",0.26400000000000001,1,"6AV63331GA000AX0"]
["6AV6333-1HA00-0AX0","SIMATIC WinCC Premium Packaging Add-on voucher for 1 compatibility test, 1 catalog entry and 1 year CS support",2643,"ST",1,"SIMATIC",0.2,1,"6AV63331HA000AX0"]
["6AV6361-1AA01-4AA0","Process Historian 2014 SP3 Basic Package, runtime software, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 7 languages (de,en,fr,es,it,zh,ja), Executable in Windows Server 2008 R2+SP1 (64-bit)/ Server 2012 (64-bit) ******************************* Content: Set (1x DVD + 1x USB)",8980,"ST",1,"SIMATIC",0.20399999999999999,1,"6AV63611AA014AA0"]
["6AV6361-1AA01-4AE0","Process Historian 2014 SP3 Upgrade from BSC PCK 2013 or CAS 7.0 SP3 to BSC PCK 2014 SP3, runtime software, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 7 languages (de,en,fr,es,it,zh,ja), Executable in Windows Server 2008 R2+SP1 (64-bit)/ Server 2012 (64-bit) ******************************* Content: Set (1x DVD + 1x USB)",1488,"ST",1,"SIMATIC",0.20399999999999999,1,"6AV63611AA014AE0"]
["6AV6361-1AA01-4AH0","Process Historian 2014 SP3 Basic Package, runtime software, single license, SW and license key download Class A, 7 languages (de,en,fr,es,it,zh,ja), executable in Windows Server 2008 R2+SP1 (64 bit)/ Server 2012 (64 bit) ******************************* E-mail address required for delivery",8364,"ST",1,"SIMATIC",1E-3,1,"6AV63611AA014AH0"]
["6AV6361-1AA01-4AK0","Process Historian 2014 SP3 Upgrade from BSC PCK 2013 or CAS 7.0 SP3 to BSC PCK 2014 SP3, runtime software, single license, SW and license key download Class A, 7 languages (de,en,fr,es,it,zh,ja), executable in Windows Server 2008 R2+SP1 (64 bit)/ Server 2012 (64 bit) ******************************* E-mail address required for delivery",1323,"ST",1,"SIMATIC",1E-3,1,"6AV63611AA014AK0"]
["6AV6361-1BA01-4AA0","Process Historian 2014 SP3 Redundancy package R-SW, single license for 2 installations SW and documentation on DVD, license key on USB flash drive, Class A, 7 languages (de,en,fr,es,it,zh,ja), Executable in Windows Server 2008 R2+SP1 (64-bit)/ Server 2012 (64-bit) ******************************* Content: Set (1x DVD + 1x USB)",16082,"ST",1,"SIMATIC",0.20499999999999999,1,"6AV63611BA014AA0"]
["6AV6361-1BA01-4AH0","Process Historian 2014 SP3 Redundancy package R-SW, single license for 2 installations SW and license key download Class A, 7 languages (de,en,fr,es,it,zh,ja), executable in Windows Server 2008 R2+SP1 (64 bit)/ Server 2012 (64 bit) ******************************* E-mail address required for delivery",14980,"ST",1,"SIMATIC",1E-3,1,"6AV63611BA014AH0"]
["6AV6361-1CA00-0AD0","Process Historian Option Redundancy for BSC PCK, Runtime software, single license, License key on USB flash drive ******************************* Content: 1x USB",1746,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63611CA000AD0"]
["6AV6361-1CA00-0AJ0","Process Historian Option Redundancy for BSC PCK, Runtime software, Single license, License key download ******************************* E-mail address required for delivery",1626,"ST",1,"SIMATIC",1E-3,1,"6AV63611CA000AJ0"]
["6AV6361-1HA01-4AB0","Proc Historian OPC UA Serv OPT for Process Historian 2014 SP3, runtime software, single license, license key on USB flash drive ******************************* Content: 1x USB",2551,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63611HA014AB0"]
["6AV6361-1HA01-4AJ0","Proc Historian OPC UA Serv OPT for Process Historian 2014 SP3, runtime software, Single license, SW and License Key Download ******************************* E-mail address required for delivery",2376,"ST",1,"SIMATIC",1E-3,1,"6AV63611HA014AJ0"]
["6AV6361-2AA01-4AA0","Information Server 2014 SP3 Basic Package, runtime software, single license, incl. 3 licenses for client access, incl. 1 license f. data source acc., SW and documentation on DVD, license key on USB flash drive, Class A, 7 languages (de,en,fr,es,it,zh,ja), executable in Windows 7 Prof/Ent/Ult +SP1 (32 bit)/ 7 Prof/Ent/Ult +SP1 (64 bit)/ 8.1 Std/Prof/Ent/Ult (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 (64 bit)",3286,"ST",1,"SIMATIC",0.20399999999999999,1,"6AV63612AA014AA0"]
["6AV6361-2AA01-4AE0","Information Server 2014 SP3 Upgrade from BSC PCK 2013 to 2014 SP3 runtime software, single license, incl. 3 licenses for client access, incl. 1 license f. data source acc., SW and documentation on DVD, license key on USB flash drive, Class A, 7 languages (de,en,fr,es,it,zh,ja), executable in Windows 7 Prof/Ent/Ult +SP1 (32 bit)/ 7 Prof/Ent/Ult +SP1 (64 bit)/ 8.1 Std/Prof/Ent/Ult (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 (64 bit)",453,"ST",1,"SIMATIC",0.20399999999999999,1,"6AV63612AA014AE0"]
["6AV6361-2AA01-4AH0","Information Server 2014 SP3 Basic Package, runtime software, single license, incl. 3 licenses for client access, incl. 1 license f. data source acc., SW and license key download Class A, 7 languages (de,en,fr,es,it,zh,ja), executable in Windows 7 Prof/Ent/Ult +SP1 (32 bit)/ 7 Prof/Ent/Ult +SP1 (64 bit)/ 8.1 Std/Prof/Ent/Ult (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 (64 bit) ******************************* E-mail address required for delivery",3061,"ST",1,"SIMATIC",1E-3,1,"6AV63612AA014AH0"]
["6AV6361-2AA01-4AK0","Information Server 2014 SP3 upgrade from BSC PCK 2013 to 2014 SP3, runtime software, single license, incl. 3 licenses for client access, incl. 1 license f. data source acc., SW and license key download Class A, 7 languages (de,en,fr,es,it,zh,ja), executable in Windows 7 Prof/Ent/Ult +SP1 (32 bit)/ 7 Prof/Ent/Ult +SP1 (64 bit)/ 8.1 Std/Prof/Ent/Ult (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 (64 bit) ******************************* E-mail address required for delivery",403,"ST",1,"SIMATIC",1E-3,1,"6AV63612AA014AK0"]
["6AV6361-2BD00-0AD0","Information Server Option 1 client access, Runtime software, 1 single license Type count relevant, License key on USB flash drive ******************************* Content: 1x USB",548,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63612BD000AD0"]
["6AV6361-2BD00-0AJ0","Information Server Option 1 client access, Runtime software, 1 single license Type count relevant, License key download ******************************* E-mail address required for delivery",510,"ST",1,"SIMATIC",1E-3,1,"6AV63612BD000AJ0"]
["6AV6361-2BE00-0AD0","Information Server Option 3 client accesses, Runtime software, 3 single licenses Type count relevant, License key on USB flash drive ******************************* Content: 1x USB",1514,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63612BE000AD0"]
["6AV6361-2BE00-0AJ0","Information Server Option 3 client accesses, Runtime software, 3 Single Licenses Type count relevant, License key download ******************************* E-mail address required for delivery",1453,"ST",1,"SIMATIC",1E-3,1,"6AV63612BE000AJ0"]
["6AV6361-2BF00-0AD0","Information Server Option 5 client accesses, Runtime software, 5 single licenses Type count relevant, License key on USB flash drive ******************************* Content: 1x USB",2392,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63612BF000AD0"]
["6AV6361-2BF00-0AJ0","Information Server Option 5 client accesses, Runtime software, 5 single licenses Type count relevant, License key download ******************************* E-mail address required for delivery",2228,"ST",1,"SIMATIC",1E-3,1,"6AV63612BF000AJ0"]
["6AV6361-2BG00-0AD0","Information Server Option 10 client accesses, Runtime software, 10 single licenses Type count relevant, License key on USB flash drive ******************************* Content: 1x USB",4100,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63612BG000AD0"]
["6AV6361-2BG00-0AJ0","Information Server Option 10 client accesses, Runtime software, 10 single licenses Type count relevant, License key download ******************************* E-mail address required for delivery",3818,"ST",1,"SIMATIC",1E-3,1,"6AV63612BG000AJ0"]
["6AV6361-2CD00-0AD0","Information Server Option 1 DataSource access, Runtime software, 1 single license Type count relevant, License key on USB flash drive ******************************* Content: 1x USB",536,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63612CD000AD0"]
["6AV6361-2CD00-0AJ0","Information Server Option 1 DataSource access, Runtime software, 1 single license Type count relevant, License key download ******************************* E-mail address required for delivery",499,"ST",1,"SIMATIC",1E-3,1,"6AV63612CD000AJ0"]
["6AV6361-2CE00-0AD0","Information Server Option 3 DataSource accesses, Runtime software, 3 single licenses Type count relevant, License key on USB flash drive ******************************* Content: 1x USB",1339,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63612CE000AD0"]
["6AV6361-2CE00-0AJ0","Information Server Option 3 DataSource accesses, Runtime software, 3 Single Licenses Type count relevant, License key download ******************************* E-mail address required for delivery",1248,"ST",1,"SIMATIC",1E-3,1,"6AV63612CE000AJ0"]
["6AV6362-1AB00-0AH0","SIMATIC WinCC/Web Navigator, 1 client license (countable), Option f. WinCC V7.4 or higher and WinCC Prof. V14 or higher, runtime software, Single license, License key download ******************************* E-mail address required for delivery",3262,"ST",1,"SIMATIC",1E-3,1,"6AV63621AB000AH0"]
["6AV6362-1AB00-0BB0","SIMATIC WinCC/Web Navigator, 1 client license (countable), Option f. WinCC V7.4 or higher and WinCC Prof. V14 or higher, runtime software, single license, license key on USB flash drive ******************************* Content: 1x USB",3667,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63621AB000BB0"]
["6AV6362-1AD00-0AH0","SIMATIC WinCC/Web Navigator, 3 client licenses (countable), Option f. WinCC V7.4 or higher and WinCC Prof. V14 or higher, runtime software, Single license, License key download ******************************* E-mail address required for delivery",6736,"ST",1,"SIMATIC",1E-3,1,"6AV63621AD000AH0"]
["6AV6362-1AD00-0BB0","SIMATIC WinCC/Web Navigator, 3 client licenses (countable), Option f. WinCC V7.4 or higher and WinCC Prof. V14 or higher, runtime software, single license, license key on USB flash drive ******************************* Content: 1x USB",7575,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63621AD000BB0"]
["6AV6362-1AF00-0AH0","SIMATIC WinCC/Web Navigator, 10 client licenses (countable), Option f. WinCC V7.4 or higher and WinCC Prof. V14 or higher, runtime software, Single license, License key download ******************************* E-mail address required for delivery",11760,"ST",1,"SIMATIC",1E-3,1,"6AV63621AF000AH0"]
["6AV6362-1AF00-0BB0","SIMATIC WinCC/Web Navigator, 10 client licenses (countable), Option f. WinCC V7.4 or higher and WinCC Prof. V14 or higher, runtime software, single license, license key on USB flash drive ******************************* Content: 1x USB",13225,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63621AF000BB0"]
["6AV6362-1AJ00-0AH0","SIMATIC WinCC/Web Navigator, 30 client licenses (countable), Option f. WinCC V7.4 or higher and WinCC Prof. V14 or higher, runtime software, Single license, License key download ******************************* E-mail address required for delivery",28875,"ST",1,"SIMATIC",1E-3,1,"6AV63621AJ000AH0"]
["6AV6362-1AJ00-0BB0","SIMATIC WinCC/Web Navigator, 30 client licenses (countable), Option f. WinCC V7.4 or higher and WinCC Prof. V14 or higher, runtime software, single license, license key on USB flash drive ******************************* Content: 1x USB",32472,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63621AJ000BB0"]
["6AV6362-1AM00-0AH0","SIMATIC WinCC/Web Navigator, 100 client licenses (countable) Option f. WinCC V7.4 or higher and WinCC Prof. V14 or higher, runtime software, Single license, License key download ******************************* E-mail address required for delivery",59535,"ST",1,"SIMATIC",1E-3,1,"6AV63621AM000AH0"]
["6AV6362-1AM00-0BB0","SIMATIC WinCC/Web Navigator, 100 client licenses (countable) Option f. WinCC V7.4 or higher and WinCC Prof. V14 or higher, runtime software, single license, license key on USB flash drive ******************************* Content: 1x USB",66951,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63621AM000BB0"]
["6AV6362-1BA00-0AH0","SIMATIC WinCC/Web Navigator, Diagnostic Client license, Option f. WinCC V7.4 or higher and WinCC Prof. V14 or higher, runtime software, Single license, License key download ******************************* E-mail address required for delivery",3262,"ST",1,"SIMATIC",1E-3,1,"6AV63621BA000AH0"]
["6AV6362-1BA00-0BB0","SIMATIC WinCC/Web Navigator, Diagnostic Client license, Option f. WinCC V7.4 or higher and WinCC Prof. V14 or higher, runtime software, single license, license key on USB flash drive ******************************* Content: 1x USB",3667,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63621BA000BB0"]
["6AV6362-1FA00-0AH0","SIMATIC WinCC/Web Navigator, Load balancing, licenses for 2 web servers, Option for WinCC V7.4 or higher, runtime software, Single license, License key download ******************************* E-mail address required for delivery",3436,"ST",1,"SIMATIC",1E-3,1,"6AV63621FA000AH0"]
["6AV6362-1FA00-0BB0","SIMATIC WinCC/Web Navigator, Load balancing, licenses for 2 web servers, Option for WinCC V7.4 or higher, runtime software, single license, License key on USB flash drive ******************************* Content: 1x USB",3864,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63621FA000BB0"]
["6AV6362-1GA00-0AH0","SIMATIC WinCC/Web Navigator, load balancing set up, licenses for 2 web servers to 2 redundant WinCC systems, Option for WinCC V7.4 or higher, runtime software, Single license, License key download ******************************* E-mail address required for delivery",1113,"ST",1,"SIMATIC",1E-3,1,"6AV63621GA000AH0"]
["6AV6362-1GA00-0BB0","SIMATIC WinCC/Web Navigator, load balancing step up, licenses for 2 web servers to 2 redundant WinCC systems, Option for WinCC V7.4 or higher, runtime software, single license, License key on USB flash drive ******************************* Content: 1x USB",1252,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63621GA000BB0"]
["6AV6362-2AB00-0AH0","SIMATIC WinCC/WEBUX Monitor, 1 client license (countable), Option f. WinCC V7.3 or higher and WinCC Prof. V14 or higher, runtime software, Single license, License key download, Server-end Windows 64 bit required ******************************* E-mail address required for delivery",525,"ST",1,"SIMATIC",1E-3,1,"6AV63622AB000AH0"]
["6AV6362-2AB00-0BB0","SIMATIC WinCC/WebUX Monitor, 1 client license (countable), Option f. WinCC V7.3 or higher and WinCC Prof. V14 or higher, runtime software, single license, license key on USB flash drive, Windows 64-bit on the server side required ******************************* Content: 1x USB",591,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63622AB000BB0"]
["6AV6362-2AD00-0AH0","SIMATIC WinCC/WEBUX Monitor, 3 client licenses (countable), Option f. WinCC V7.3 or higher and WinCC Prof. V14 or higher, runtime software, Single license, License key download, Server-end Windows 64 bit required ******************************* E-mail address required for delivery",1470,"ST",1,"SIMATIC",1E-3,1,"6AV63622AD000AH0"]
["6AV6362-2AD00-0BB0","SIMATIC WinCC/WebUX Monitor, 3 client licenses (countable), Option f. WinCC V7.3 or higher and WinCC Prof. V14 or higher, runtime software, single license, license key on USB flash drive, Windows 64-bit on the server side required ******************************* Content: 1x USB",1654,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63622AD000BB0"]
["6AV6362-2AF00-0AH0","SIMATIC WinCC/WEBUX Monitor, 10 client licenses (countable), Option f. WinCC V7.3 or higher and WinCC Prof. V14 or higher, runtime software, Single license, License key download, Server-end Windows 64 bit required ******************************* E-mail address required for delivery",3518,"ST",1,"SIMATIC",1E-3,1,"6AV63622AF000AH0"]
["6AV6362-2AF00-0BB0","SIMATIC WinCC/WebUX Monitor, 10 client licenses (countable), Option f. WinCC V7.3 or higher and WinCC Prof. V14 or higher, runtime software, single license, license key on USB flash drive, Windows 64-bit on the server side required ******************************* Content: 1x USB",3957,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63622AF000BB0"]
["6AV6362-2AJ00-0AH0","SIMATIC WinCC/WEBUX Monitor, 30 client licenses (countable), Option f. WinCC V7.3 or higher and WinCC Prof. V14 or higher, runtime software, Single license, License key download, Server-end Windows 64 bit required ******************************* E-mail address required for delivery",8610,"ST",1,"SIMATIC",1E-3,1,"6AV63622AJ000AH0"]
["6AV6362-2AJ00-0BB0","SIMATIC WinCC/WebUX Monitor, 30 client licenses (countable), Option f. WinCC V7.3 or higher and WinCC Prof. V14 or higher, runtime software, single license, license key on USB flash drive, Windows 64-bit on the server side required ******************************* Content: 1x USB",9684,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63622AJ000BB0"]
["6AV6362-2AM00-0AH0","SIMATIC WinCC/WEBUX Monitor, 100 client licenses (countable) Option f. WinCC V7.3 or higher and WinCC Prof. V14 or higher, runtime software, Single license, License key download, Server-end Windows 64 bit required ******************************* E-mail address required for delivery",19845,"ST",1,"SIMATIC",1E-3,1,"6AV63622AM000AH0"]
["6AV6362-2AM00-0BB0","SIMATIC WinCC/WebUX Monitor, 100 client licenses (countable) Option f. WinCC V7.3 or higher and WinCC Prof. V14 or higher, runtime software, single license, license key on USB flash drive, Windows 64-bit on the server side required ******************************* Content: 1x USB",22317,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63622AM000BB0"]
["6AV6362-2BB00-0AH0","SIMATIC WinCC/WEBUX Operate, 1 client license (countable), Option f. WinCC V7.3 or higher and WinCC Prof. V14 or higher, runtime software, Single license, License key download, Server-end Windows 64 bit required ******************************* E-mail address required for delivery",1575,"ST",1,"SIMATIC",1E-3,1,"6AV63622BB000AH0"]
["6AV6362-2BB00-0BB0","SIMATIC WinCC/WebUX Operate, 1 client license (countable), Option f. WinCC V7.3 or higher and WinCC Prof. V14 or higher, runtime software, single license, license key on USB flash drive, Windows 64-bit on the server side required ******************************* Content: 1x USB",1772,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63622BB000BB0"]
["6AV6362-2BD00-0AH0","SIMATIC WinCC/WEBUX Operate, 3 client licenses (countable), Option f. WinCC V7.3 or higher and WinCC Prof. V14 or higher, runtime software, Single license, License key download, Server-end Windows 64 bit required ******************************* E-mail address required for delivery",4410,"ST",1,"SIMATIC",1E-3,1,"6AV63622BD000AH0"]
["6AV6362-2BD00-0BB0","SIMATIC WinCC/WebUX Operate, 3 client licenses (countable), Option f. WinCC V7.3 or higher and WinCC Prof. V14 or higher, runtime software, single license, license key on USB flash drive, Windows 64-bit on the server side required ******************************* Content: 1x USB",4961,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63622BD000BB0"]
["6AV6362-2BF00-0AH0","SIMATIC WinCC/WEBUX Operate, 10 client licenses (countable), Option f. WinCC V7.3 or higher and WinCC Prof. V14 or higher, runtime software, Single license, License key download, Server-end Windows 64 bit required ******************************* E-mail address required for delivery",10500,"ST",1,"SIMATIC",1E-3,1,"6AV63622BF000AH0"]
["6AV6362-2BF00-0BB0","SIMATIC WinCC/WebUX Operate, 10 client licenses (countable), Option f. WinCC V7.3 or higher and WinCC Prof. V14 or higher, runtime software, single license, license key on USB flash drive, Windows 64-bit on the server side required ******************************* Content: 1x USB",11809,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63622BF000BB0"]
["6AV6362-2BJ00-0AH0","SIMATIC WinCC/WEBUX Operate, 30 client licenses (countable), Option f. WinCC V7.3 or higher and WinCC Prof. V14 or higher, runtime software, Single license, License key download, Server-end Windows 64 bit required ******************************* E-mail address required for delivery",25725,"ST",1,"SIMATIC",1E-3,1,"6AV63622BJ000AH0"]
["6AV6362-2BJ00-0BB0","SIMATIC WinCC/WebUX Operate, 30 client licenses (countable), Option f. WinCC V7.3 or higher and WinCC Prof. V14 or higher, runtime software, single license, license key on USB flash drive, Windows 64-bit on the server side required ******************************* Content: 1x USB",28929,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63622BJ000BB0"]
["6AV6362-2BM00-0AH0","SIMATIC WinCC/WEBUX Operate, 100 client licenses (countable) Option f. WinCC V7.3 or higher and WinCC Prof. V14 or higher, runtime software, Single license, License key download, Server-end Windows 64 bit required ******************************* E-mail address required for delivery",59535,"ST",1,"SIMATIC",1E-3,1,"6AV63622BM000AH0"]
["6AV6362-2BM00-0BB0","SIMATIC WinCC/WebUX Operate, 100 client licenses (countable) Option f. WinCC V7.3 or higher and WinCC Prof. V14 or higher, runtime software, single license, license key on USB flash drive, Windows 64-bit on the server side required ******************************* Content: 1x USB",66951,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63622BM000BB0"]
["6AV6362-3AB00-0AH0","SIMATIC WinCC/DataMonitor, 1 client license (countable), Option for WinCC V7.4 or higher, and WinCC Prof. V14 or higher, runtime software, Single license, License key download ******************************* E-mail address required for delivery",2126,"ST",1,"SIMATIC",1E-3,1,"6AV63623AB000AH0"]
["6AV6362-3AB00-0BB0","SIMATIC WinCC/DataMonitor, 1 client license (countable), Option for WinCC V7.4 or higher, and WinCC Prof. V14 or higher, runtime software, single license, license key on USB flash drive ******************************* Content: 1x USB",2390,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63623AB000BB0"]
["6AV6362-3AD00-0AH0","SIMATIC WinCC/DataMonitor, 3 client licenses (countable), Option for WinCC V7.4 or higher, and WinCC Prof. V14 or higher, runtime software, Single license, License key download ******************************* E-mail address required for delivery",3250,"ST",1,"SIMATIC",1E-3,1,"6AV63623AD000AH0"]
["6AV6362-3AD00-0BB0","SIMATIC WinCC/DataMonitor, 3 client licenses (countable), Option for WinCC V7.4 or higher, and WinCC Prof. V14 or higher, runtime software, single license, license key on USB flash drive ******************************* Content: 1x USB",3656,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63623AD000BB0"]
["6AV6362-3AF00-0AH0","SIMATIC WinCC/DataMonitor, 10 client licenses (countable), Option for WinCC V7.4 or higher, and WinCC Prof. V14 or higher, runtime software, Single license, License key download ******************************* E-mail address required for delivery",5950,"ST",1,"SIMATIC",1E-3,1,"6AV63623AF000AH0"]
["6AV6362-3AF00-0BB0","SIMATIC WinCC/DataMonitor, 10 client licenses (countable), Option for WinCC V7.4 or higher, and WinCC Prof. V14 or higher, runtime software, single license, license key on USB flash drive ******************************* Content: 1x USB",6691,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63623AF000BB0"]
["6AV6362-3AJ00-0AH0","SIMATIC WinCC/DataMonitor, 30 client licenses (countable), Option for WinCC V7.4 or higher, and WinCC Prof. V14 or higher, runtime software, Single license, License key download ******************************* E-mail address required for delivery",12285,"ST",1,"SIMATIC",1E-3,1,"6AV63623AJ000AH0"]
["6AV6362-3AJ00-0BB0","SIMATIC WinCC/DataMonitor, 30 client licenses (countable), Option for WinCC V7.4 or higher, and WinCC Prof. V14 or higher, runtime software, single license, license key on USB flash drive ******************************* Content: 1x USB",13815,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63623AJ000BB0"]
["6AV6362-4AA07-4AA0","WinCC/IND.DATABRIDGE V7.4 SP1, Basic Package V7.4 SP1, Option for WinCC V7.4 SP1 and WinCC Prof. V14, Data exchange with databases and OPC servers, Runtime/Configuration software on CD-ROM, Single license, License key on USB stick",887,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63624AA074AA0"]
["6AV6362-4AA07-4AE0","WinCC/IND.DATABRIDGE V7.4 SP1, Upgrade from V7.X to V7.4 SP1, Option for WinCC V7.4 SP1 and WinCC Prof. V14, Data exchange with databases and OPC servers, Runtime/Configuration software on CD-ROM, Single license, License key on USB stick",349,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63624AA074AE0"]
["6AV6362-4AA07-4AH0","WinCC/IND.DATABRIDGE V7.4 SP1, Basic Package V7.4 SP1, Option for WinCC V7.4 SP1 and WinCC Prof. V14, Data exchange with databases and OPC servers, Runtime/Configuration software, Single license, SW and License Key Download ******************************* E-mail address required for delivery",788,"ST",1,"SIMATIC",1E-3,1,"6AV63624AA074AH0"]
["6AV6362-4AA07-4AK0","WinCC/IND.DATABRIDGE V7.4 SP1, Upgrade from V7.X to V7.4 SP1, Option for WinCC V7.4 SP1 and WinCC Prof. V14, Data exchange with databases and OPC servers, Runtime/Configuration software, Single license, SW and License Key Download ******************************* E-mail address required for delivery",310,"ST",1,"SIMATIC",1E-3,1,"6AV63624AA074AK0"]
["6AV6362-4AA07-5AA0","WinCC/IndustrialDataBridge V7.5, Basic Package V7.5, option for WinCC V7.5 and WinCC Prof. V15, data exchange with databases and OPC servers, runtime/configuration software on CD-ROM, single license, license key on USB flash drive Please observe product release: support.industry.siemens.com SIOS entry ID:  109759994",888,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63624AA075AA0"]
["6AV6362-4AA07-5AE0","WinCC/IndustrialDataBridge V7.5, Upgrade from V7.2/7.3 -> V7.5, option for WinCC V7.5 and WinCC Prof. V15, data exchange with databases and OPC servers, runtime/configuration software on CD-ROM, single license, license key on USB flash drive Please observe product release: support.industry.siemens.com SIOS entry ID:  109759994",494,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63624AA075AE0"]
["6AV6362-4AA07-5AE1","WinCC/IndustrialDataBridge V7.5, Upgrade from V7.4 -> V7.5, option for WinCC V7.5 and WinCC Prof. V15, data exchange with databases and OPC servers, runtime/configuration software on CD-ROM, single license, license key on USB flash drive Please observe product release: support.industry.siemens.com SIOS entry ID:  109759994",350,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63624AA075AE1"]
["6AV6362-4AA07-5AH0","WinCC/IndustrialDataBridge V7.5, Basic Package V7.5, option for WinCC V7.5 and WinCC Prof. V15, data exchange with databases and OPC servers, runtime/configuration software Single license, SW and license key download Please observe product release: support.industry.siemens.com SIOS entry ID:  109759994 ******************************* E-mail address required for delivery",788,"ST",1,"SIMATIC",1E-3,1,"6AV63624AA075AH0"]
["6AV6362-4AA07-5AK0","WinCC/IndustrialDataBridge V7.5, Upgrade from V7.2/7.3 -> V7.5, option for WinCC V7.5 and WinCC Prof. V15, data exchange with databases and OPC servers, runtime/configuration software Single license, SW and license key download Please observe product release: support.industry.siemens.com SIOS entry ID:  109759994 ******************************* E-mail address required for delivery",439,"ST",1,"SIMATIC",1E-3,1,"6AV63624AA075AK0"]
["6AV6362-4AA07-5AK1","WinCC/IndustrialDataBridge V7.5, Upgrade from V7.4 -> V7.5, option for WinCC V7.5 and WinCC Prof. V15, data exchange with databases and OPC servers, runtime/configuration software Single license, SW and license key download Please observe product release: support.industry.siemens.com SIOS entry ID:  109759994 ******************************* E-mail address required for delivery",310,"ST",1,"SIMATIC",1E-3,1,"6AV63624AA075AK1"]
["6AV6362-4AD00-0AH0","WinCC/Industrial-Data-Bridge, 300 tags (countable), Option for WinCC V7.4 or higher, and WinCC Prof. V14 or higher, Data exchange with databases and OPC servers, runtime software, Single license, License key download ******************************* E-mail address required for delivery",945,"ST",1,"SIMATIC",1E-3,1,"6AV63624AD000AH0"]
["6AV6362-4AD00-0BB0","WinCC/Industrial-Data-Bridge, 300 tags (countable), Option for WinCC V7.4 or higher, and WinCC Prof. V14 or higher, Data exchange with databases and OPC servers, runtime software, single license, License key on USB flash drive ******************************* Content: 1x USB",1063,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63624AD000BB0"]
["6AV6362-4AF00-0AH0","WinCC/Industrial-Data-Bridge, 1000 tags (countable), Option for WinCC V7.4 or higher, and WinCC Prof. V14 or higher, Data exchange with databases and OPC servers, runtime software, Single license, License key download ******************************* E-mail address required for delivery",2100,"ST",1,"SIMATIC",1E-3,1,"6AV63624AF000AH0"]
["6AV6362-4AF00-0BB0","WinCC/Industrial-Data-Bridge, 1000 tags (countable), Option for WinCC V7.4 or higher, and WinCC Prof. V14 or higher, Data exchange with databases and OPC servers, runtime software, single license, License key on USB flash drive ******************************* Content: 1x USB",2362,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63624AF000BB0"]
["6AV6362-4AH00-0AH0","WinCC/Industrial-Data-Bridge, 3000 tags (countable), Option for WinCC V7.4 or higher, and WinCC Prof. V14 or higher, Data exchange with databases and OPC servers, runtime software, Single license, License key download ******************************* E-mail address required for delivery",3150,"ST",1,"SIMATIC",1E-3,1,"6AV63624AH000AH0"]
["6AV6362-4AH00-0BB0","WinCC/Industrial-Data-Bridge, 3000 tags (countable), Option for WinCC V7.4 or higher, and WinCC Prof. V14 or higher, Data exchange with databases and OPC servers, runtime software, single license, License key on USB flash drive ******************************* Content: 1x USB",3543,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63624AH000BB0"]
["6AV6362-5AA07-5AH0","WinCC/Cloud Connect V7.5 Option for WinCC V7.5, runtime software, single license, license key download ******************************* E-mail address required for delivery",310,"ST",1,"SIMATIC",1E-3,1,"6AV63625AA075AH0"]
["6AV6362-5AA07-5BB0","WinCC/Cloud Connect V7.5 Option for WinCC V7.5, runtime software, single license, License key on USB flash drive ******************************* Content: 1x USB",349,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63625AA075BB0"]
["6AV6371-1CA07-0AQ0","EPL Royalty for WinCC V7, Server operation option only valid in connection with Enterprise License agreement, requires EPL Master",3302,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV63711CA070AQ0"]
["6AV6371-1CA07-4AX0","SIMATIC WinCC/Server V7.4, Option for WinCC V7.4, runtime software, single license, License key on USB flash drive ******************************* Content: 1x USB",3712,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63711CA074AX0"]
["6AV6371-1CA07-5AX0","SIMATIC WinCC/Server V7.5, Option for WinCC V7.5, runtime software, single license, License key on USB flash drive ******************************* Content: 1x USB",3713,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63711CA075AX0"]
["6AV6371-1CB07-0AQ0","EPL Royalty for WinCC V7, User Archives option. only valid in connection with Enterprise License agreement, requires EPL Master",816,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV63711CB070AQ0"]
["6AV6371-1CB07-4AX0","WinCC/User-Archives V7.4, Option for WinCC V7.4, runtime software, single license, License key on USB flash drive ******************************* Content: 1x USB",918,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63711CB074AX0"]
["6AV6371-1CB07-5AX0","WinCC/User-Archives V7.5, Option for WinCC V7.5, runtime software, single license, License key on USB flash drive ******************************* Content: 1x USB",918,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63711CB075AX0"]
["6AV6371-1CC07-0AX4","SIMATIC WinCC/ODK Upgrade Open Development Kit, Upgrade to V7.0, for C-programming, for SIMATIC WinCC V7.0, V6.X, V5.X, single license",396,"ST",1,"SIMATIC",0.129,1,"6AV63711CC070AX4"]
["6AV6371-1CC07-4AX0","SIMATIC WinCC/ODK V7.4, Open Development Kit, Option for SIMATIC WinCC V7.4 for C-programming, software on CD-ROM ******************************* Content: 1x DVD",1518,"ST",1,"SIMATIC",0.183,1,"6AV63711CC074AX0"]
["6AV6371-1CC07-5AX0","SIMATIC WinCC/ODK V7.5, Open Development Kit, option for SIMATIC WinCC V7.5 for C-programming, software on CD-ROM ******************************* Content: 1x DVD",1518,"ST",1,"SIMATIC",0.183,1,"6AV63711CC075AX0"]
["6AV6371-1CF07-0AQ0","EPL Royalty for WinCC V7, Option redundancy only valid in connection with Enterprise License agreement, requires EPL Master",3431,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV63711CF070AQ0"]
["6AV6371-1CF07-4AX0","SIMATIC WinCC/Redundancy V7.4, Option for SIMATIC WinCC V7.4, Runtime software, Single License for 2 installations ******************************* Content: 1x USB",3858,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63711CF074AX0"]
["6AV6371-1CF07-5AX0","SIMATIC WinCC/Redundancy V7.5, option for SIMATIC WinCC V7.5, Runtime software, Single License for 2 installations ******************************* Content: 1x USB",3858,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63711CF075AX0"]
["6AV6371-1DG07-0AQ0","EPL Royalty for WinCC V7, Option pro/Agent only valid in connection with Enterprise License agreement, requires EPL Master",996,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV63711DG070AQ0"]
["6AV6371-1DG07-4AX0","SIMATIC WinCC/ProAgent V7.4, process diagnostics based on S7-Graph and S7-PDIAG, option for SIMATIC/WinCC V7.4, runtime software, single license, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",1120,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63711DG074AX0"]
["6AV6371-1DG07-4AX3","WinCC/ProAgent upgrade from V7.X to V7.4 for SIMATIC WinCC V7.4, Runtime software on CD-ROM, Single license license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",197,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63711DG074AX3"]
["6AV6371-1DG07-5AX0","SIMATIC WinCC/ProAgent V7.5, process diagnostics based on S7-Graph and S7-PDIAG, option for SIMATIC/WinCC V7.5, runtime software, single license, software on CD license key on USB flash drive Please observe product release: support.industry.siemens.com SIOS entry ID:  109759995 ******************************* Content: Set (1x DVD + 1x USB)",1120,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63711DG075AX0"]
["6AV6371-1DG07-5AX3","WinCC/ProAgent upgrade from V7.2/7.3 -> V7.5 for SIMATIC WinCC V7.5, runtime software on CD-ROM, license key on USB flash drive Please observe product release: support.industry.siemens.com SIOS entry ID:  109759995 ******************************* Content: Set (1x DVD + 1x USB)",279,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63711DG075AX3"]
["6AV6371-1DG07-5AX4","WinCC/ProAgent upgrade from V7.4 -> V7.5 for SIMATIC WinCC V7.5, runtime software on CD-ROM, license key on USB flash drive Please observe product release: support.industry.siemens.com SIOS entry ID:  109759995 ******************************* Content: Set (1x DVD + 1x USB)",197,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63711DG075AX4"]
["6AV6371-1DH07-0DQ0","EPL Royalty for WinCC V7, Option Web Navigator Server and client components, incl. 50 client licenses. only valid in connection with Enterprise License agreement, requires EPL Master",35422,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV63711DH070DQ0"]
["6AV6371-1DH07-4AV5","Trainer Package WinCC V7.4 Asia and Web Navigator V7.4, includes: SW and documentation on DVD, 6-unit license on USB stick for WinCC V7.4 Asia RC 2048, Web Navigator for educational purposes only",2689,"ST",1,"SIMATIC",0.32800000000000001,1,"6AV63711DH074AV5"]
["6AV6371-1DH07-4AX5","Trainer Package WinCC V7.4 and Web Navigator V7.4, includes: SW and documentation on DVD, 6-unit license on USB stick for WinCC V7.4 RC 2048, Web Navigator, for educational purposes only",2689,"ST",1,"SIMATIC",0.251,1,"6AV63711DH074AX5"]
["6AV6371-1DH07-5AV5","Trainer Package WinCC V7.5 Asia and Web Navigator V7.5, includes: SW and documentation on DVD, 6-unit license on USB stick for WinCC V7.5 Asia RC 2048, Web Navigator and diagnostics client, for educational purposes only",2689,"ST",1,"SIMATIC",0.378,1,"6AV63711DH075AV5"]
["6AV6371-1DH07-5AX5","Trainer Package WinCC V7.5 and Web Navigator V7.5, includes: SW and documentation on DVD, 6-unit license on USB stick for WinCC V7.5 RC 2048, Web Navigator and diagnostics client, for educational purposes only",2689,"ST",1,"SIMATIC",0.30099999999999999,1,"6AV63711DH075AX5"]
["6AV6371-1DQ17-0AX0","SIMATIC WinCC/Archive 1500, 1500 archive tags for SIMATIC WinCC V7.0, Runtime software, Single license, count relevant",3084,"ST",1,"SIMATIC",9.1999999999999998E-2,1,"6AV63711DQ170AX0"]
["6AV6371-1DQ17-0BX0","SIMATIC WinCC/Archive 5000, 5000 archive tags for SIMATIC WinCC V7.0, Runtime software, Single license, count relevant",10322,"ST",1,"SIMATIC",9.1999999999999998E-2,1,"6AV63711DQ170BX0"]
["6AV6371-1DQ17-0CX0","SIMATIC WinCC/Archive 10000, 10000 archive tags for SIMATIC WinCC V7.0, Runtime software, Single license, count relevant",16088,"ST",1,"SIMATIC",9.1999999999999998E-2,1,"6AV63711DQ170CX0"]
["6AV6371-1DQ17-0EX0","SIMATIC WinCC/Archive 30000, 30000 archive tags for SIMATIC WinCC V7.0, Runtime software, Single license, count relevant",26142,"ST",1,"SIMATIC",9.1999999999999998E-2,1,"6AV63711DQ170EX0"]
["6AV6371-1DQ17-0GX0","SIMATIC WinCC/Archive 80000, 80000 archive tags for SIMATIC WinCC V7.0, Runtime software, Single license, count relevant",65688,"ST",1,"SIMATIC",9.1999999999999998E-2,1,"6AV63711DQ170GX0"]
["6AV6371-1DQ17-0JX0","SIMATIC WinCC/Archive 120000, 120000 archive tags for SIMATIC WinCC V7.0, Runtime software, Single license, count relevant",77749,"ST",1,"SIMATIC",9.1999999999999998E-2,1,"6AV63711DQ170JX0"]
["6AV6371-1DQ17-0XV3","SIMATIC WinCC/CAS Upgrade Central Archive Server V6.2-> V7.0 SP3 Asia, Option for WinCC V7.0 SP3 Asia runtime software, single license",1583,"ST",1,"SIMATIC",0.28399999999999997,1,"6AV63711DQ170XV3"]
["6AV6371-1DQ17-0XX3","SIMATIC WinCC/CAS Upgrade Central Archive Server V6.2-> V7.0 SP3 Option for WinCC V7.0 SP3, runtime software, single license",1583,"ST",1,"SIMATIC",0.27200000000000002,1,"6AV63711DQ170XX3"]
["6AV6371-1DQ17-4AX0","SIMATIC WinCC/Archive V7.4, 1500 archive variables (countable) Option for WinCC V7.4 runtime software, single license, License key on USB flash drive ******************************* Content: 1x USB",2908,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63711DQ174AX0"]
["6AV6371-1DQ17-4BX0","SIMATIC WinCC/Archive V7.4, 5000 archive variables (countable) Option for WinCC V7.4 runtime software, single license, License key on USB flash drive ******************************* Content: 1x USB",9738,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63711DQ174BX0"]
["6AV6371-1DQ17-4CX0","SIMATIC WinCC/Archive V7.4, 10000 archive variables (countable) Option for WinCC V7.4 runtime software, single license, License key on USB flash drive ******************************* Content: 1x USB",15174,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63711DQ174CX0"]
["6AV6371-1DQ17-4EX0","SIMATIC WinCC/Archive V7.4, 30000 archive variables (countable) Option for WinCC V7.4 runtime software, single license, License key on USB flash drive ******************************* Content: 1x USB",24662,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63711DQ174EX0"]
["6AV6371-1DQ17-5AX0","SIMATIC WinCC/Archive V7.5, 1500 Archive Tags (countable) Option for WinCC V7.5 Runtime software, single license, license key on USB flash drive ******************************* Content: 1x USB",2909,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63711DQ175AX0"]
["6AV6371-1DQ17-5BX0","SIMATIC WinCC/Archive V7.5, 5000 Archive Tags (countable) option for WinCC V7.5 runtime software, single license, license key on USB flash drive",9738,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63711DQ175BX0"]
["6AV6371-1DQ17-5CX0","SIMATIC WinCC/Archive V7.5, 10000 Archive Tags (countable) option for WinCC V7.5 runtime software, single license, license key on USB flash drive",15174,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63711DQ175CX0"]
["6AV6371-1DQ17-5EX0","SIMATIC WinCC/Archive V7.5, 30000 Archive Tags (countable) option for WinCC V7.5 runtime software, single license, license key on USB flash drive",24662,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63711DQ175EX0"]
["6AV6371-1DR07-0AQ0","EPL Royalty for WinCC V7, Option Connectivity Pack only valid in connection with Enterprise License agreement, requires EPL Master",1113,"ST",1,"SIMATIC",1.2999999999999999E-2,1,"6AV63711DR070AQ0"]
["6AV6371-1DR07-4AX0","WinCC/Connectivity Pack V7.4, Option for WinCC V7.4, runtime software, single license, License key on USB flash drive ******************************* Content: 1x USB",1252,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63711DR074AX0"]
["6AV6371-1DR07-5AX0","WinCC/Connectivity Pack V7.5, Option for WinCC V7.5, runtime software, single license, License key on USB flash drive ******************************* Content: 1x USB",1252,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63711DR075AX0"]
["6AV6371-1DR17-4AX0","WinCC/Connectivity Station V7.4 Option for WinCC V7.4, runtime software, single license, License key on USB flash drive ******************************* Content: 1x USB",3542,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63711DR174AX0"]
["6AV6371-1DR17-5AX0","WinCC/Connectivity Station V7.5 Option for WinCC V7.5, runtime software, single license, License key on USB flash drive ******************************* Content: 1x USB",3542,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63711DR175AX0"]
["6AV6371-1DV07-4AX0","WinCC/Audit RT V7.4, per operator panel, generation of an audit trail, Option for WinCC V7.4, runtime software, single license, SW and documentation on CD, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",860,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV63711DV074AX0"]
["6AV6371-1DV07-4BX3","WinCC/Audit RT Upgrade from V7.X to V7.4 for WinCC/Audit RT, runtime software, single license, SW and documentation on CD, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",191,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV63711DV074BX3"]
["6AV6371-1DV07-5AX0","WinCC/Audit RT V7.5, per operator panel, generation of an audit trail, Option for WinCC V7.5, runtime software, single license, SW and documentation on CD, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",861,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV63711DV075AX0"]
["6AV6371-1DV07-5BX3","WinCC/Audit RT Upgrade from V7.2/7.3 -> V7.5 for WinCC/Audit RT, runtime software, single license, SW and documentation on CD, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",191,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV63711DV075BX3"]
["6AV6371-1DV07-5BX4","WinCC/Audit RT Upgrade from V7.4 -> V7.5 for WinCC/Audit RT, runtime software, single license, SW and documentation on CD, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",127,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV63711DV075BX4"]
["6AV6371-1DV17-4AX0","WinCC/Audit RC V7.4 for configuration of the Audit Trail (RT and eng.) with Versioning, incl. RT license, Option for WinCC V7.4, Runtime/configuration software on CD-ROM, single license, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",7588,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV63711DV174AX0"]
["6AV6371-1DV17-4BX3","SIMATIC WinCC/Audit RC Upgrade from V7.X to V7.4 for WinCC/Audit RC, and WinCC/Change-Control, Runtime/configuration software on CD-ROM, single license, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",949,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV63711DV174BX3"]
["6AV6371-1DV17-5AX0","WinCC/Audit RC V7.5 for configuration of the Audit Trail (RT and eng.) with Versioning, incl. RT license, Option for WinCC V7.5, Runtime/configuration software on CD-ROM, single license, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",7589,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV63711DV175AX0"]
["6AV6371-1DV17-5BX3","WinCC/Audit RC Upgrade from V7.2/7.3 -> V7.5 for WinCC/Audit RC, and WinCC/Change-Control, Runtime/configuration software on CD-ROM, single license, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",950,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV63711DV175BX3"]
["6AV6371-1DV17-5BX4","WinCC/Audit RC Upgrade from V7.4 -> V7.5 for WinCC/Audit RC, and WinCC/Change-Control, Runtime/configuration software on CD-ROM, single license, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",633,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV63711DV175BX4"]
["6AV6371-1DV27-4AX0","WinCC/Change -Control V7.4 for configuration of the Audit Trail (English) with Versioning, incl. RT license, Option for WinCC V7.4, Runtime/configuration software on CD-ROM, single license, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",5058,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV63711DV274AX0"]
["6AV6371-1DV27-5AX0","WinCC/Change Control V7.5 for configuration of the Audit Trail (English) with Versioning, incl. RT license, Option for WinCC V7.5, Runtime/configuration software on CD-ROM, single license, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",5058,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV63711DV275AX0"]
["6AV6371-1GC07-4AX0","SIMATIC WinCC/ODK V7.4, Open Development Kit, Option for SIMATIC WinCC V7.4 for C-programming, Software download ******************************* E-mail address required for delivery",1350,"ST",1,"SIMATIC",1E-3,1,"6AV63711GC074AX0"]
["6AV6371-1GC07-5AX0","SIMATIC WinCC/ODK V7.5, open development kit, option for SIMATIC WinCC V7.5 for C-programming, software download ******************************* E-mail address required for delivery",1350,"ST",1,"SIMATIC",1E-3,1,"6AV63711GC075AX0"]
["6AV6371-1HA07-4AX0","SIMATIC WinCC/Server V7.4, Option for WinCC V7.4, runtime software, Single license, License key download ******************************* E-mail address required for delivery",3302,"ST",1,"SIMATIC",1E-3,1,"6AV63711HA074AX0"]
["6AV6371-1HA07-5AX0","SIMATIC WinCC/Server V7.5, Option for WinCC V7.5, runtime software, single license, license key download ******************************* E-mail address required for delivery",3302,"ST",1,"SIMATIC",1E-3,1,"6AV63711HA075AX0"]
["6AV6371-1HB07-4AX0","WinCC/User-Archives V7.4, Option for WinCC V7.4, runtime software, Single license, License key download ******************************* E-mail address required for delivery",816,"ST",1,"SIMATIC",1E-3,1,"6AV63711HB074AX0"]
["6AV6371-1HB07-5AX0","WinCC/User-Archives V7.5, Option for WinCC V7.5, runtime software, single license, license key download ******************************* E-mail address required for delivery",816,"ST",1,"SIMATIC",1E-3,1,"6AV63711HB075AX0"]
["6AV6371-1HF07-4AX0","SIMATIC WinCC/Redundancy V7.4, Option for WinCC V7.4, runtime software, Single license, License key download ******************************* E-mail address required for delivery",3431,"ST",1,"SIMATIC",1E-3,1,"6AV63711HF074AX0"]
["6AV6371-1HF07-5AX0","SIMATIC WinCC/Redundancy V7.5, Option for WinCC V7.5, runtime software, single license, license key download ******************************* E-mail address required for delivery",3431,"ST",1,"SIMATIC",1E-3,1,"6AV63711HF075AX0"]
["6AV6371-1HG07-4AX0","WinCC/ProAgent V7.4, Process diagnostics based on S7 GRAPH and S7 PDIAG, option for SIMATIC/WinCC V7.4, runtime software, Single license, SW and License Key Download ******************************* E-mail address required for delivery",996,"ST",1,"SIMATIC",1E-3,1,"6AV63711HG074AX0"]
["6AV6371-1HG07-5AX0","SIMATIC WinCC/ProAgent V7.5, process diagnostics based on S7 GRAPH and S7 PDIAG, option for SIMATIC/WinCC V7.5, runtime software, single license, SW and license key download Please observe product release: support.industry.siemens.com SIOS entry ID:  109759995 ******************************* E-mail address required for delivery",996,"ST",1,"SIMATIC",1E-3,1,"6AV63711HG075AX0"]
["6AV6371-1HQ17-4AX0","SIMATIC WinCC/Archive V7.4, 1500 archive tags (countable) Option for WinCC V7.4 Runtime software, Single license, License key download ******************************* E-mail address required for delivery",2587,"ST",1,"SIMATIC",1E-3,1,"6AV63711HQ174AX0"]
["6AV6371-1HQ17-4BX0","SIMATIC WinCC/Archive V7.4, 5000 archive tags (countable) Option for WinCC V7.4 Runtime software, Single license, License key download ******************************* E-mail address required for delivery",8660,"ST",1,"SIMATIC",1E-3,1,"6AV63711HQ174BX0"]
["6AV6371-1HQ17-4CX0","SIMATIC WinCC/Archive V7.4, 10000 archive tags (countable) Option for WinCC V7.4 Runtime software, Single license, License key download ******************************* E-mail address required for delivery",13493,"ST",1,"SIMATIC",1E-3,1,"6AV63711HQ174CX0"]
["6AV6371-1HQ17-4EX0","SIMATIC WinCC/Archive V7.4, 30000 archive tags (countable) Option for WinCC V7.4 Runtime software, Single license, License key download ******************************* E-mail address required for delivery",21930,"ST",1,"SIMATIC",1E-3,1,"6AV63711HQ174EX0"]
["6AV6371-1HQ17-5AX0","SIMATIC WinCC/Archive V7.5, 1500 Archive Tags (countable) option for WinCC V7.5 runtime software, single license, license key download ******************************* E-mail address required for delivery",2587,"ST",1,"SIMATIC",1E-3,1,"6AV63711HQ175AX0"]
["6AV6371-1HQ17-5BX0","SIMATIC WinCC/Archive V7.5, 5000 Archive Tags (countable) option for WinCC V7.5 runtime software, single license, license key download ******************************* E-mail address required for delivery",8660,"ST",1,"SIMATIC",1E-3,1,"6AV63711HQ175BX0"]
["6AV6371-1HQ17-5CX0","SIMATIC WinCC/Archive V7.5, 10000 Archive Tags (countable) option for WinCC V7.5 runtime software, single license, license key download ******************************* E-mail address required for delivery",13493,"ST",1,"SIMATIC",1E-3,1,"6AV63711HQ175CX0"]
["6AV6371-1HQ17-5EX0","SIMATIC WinCC/Archive V7.5, 30000 Archive Tags (countable) option for WinCC V7.5 runtime software, single license, license key download ******************************* E-mail address required for delivery",21930,"ST",1,"SIMATIC",1E-3,1,"6AV63711HQ175EX0"]
["6AV6371-1HR07-4AX0","WinCC/Connectivity Pack V7.4, Option for WinCC V7.4, runtime software, Single license, License key download ******************************* E-mail address required for delivery",1113,"ST",1,"SIMATIC",1E-3,1,"6AV63711HR074AX0"]
["6AV6371-1HR07-5AX0","WinCC/Connectivity Pack V7.5, Option for WinCC V7.5, runtime software, single license, license key download ******************************* E-mail address required for delivery",1113,"ST",1,"SIMATIC",1E-3,1,"6AV63711HR075AX0"]
["6AV6371-1HR17-4AX0","WinCC/Connectivity Station V7.4 Option for WinCC V7.4, runtime software, Single license, License key download ******************************* E-mail address required for delivery",3149,"ST",1,"SIMATIC",1E-3,1,"6AV63711HR174AX0"]
["6AV6371-1HR17-5AX0","WinCC/Connectivity Station V7.5 Option for WinCC V7.5, runtime software, single license, license key download ******************************* E-mail address required for delivery",3149,"ST",1,"SIMATIC",1E-3,1,"6AV63711HR175AX0"]
["6AV6371-1HV07-4AX0","WinCC/Audit RT V7.4, per operator panel, generation of an audit trail, Option for WinCC V7.4, runtime software, Single license, SW and License Key Download ******************************* E-mail address required for delivery",766,"ST",1,"SIMATIC",1E-3,1,"6AV63711HV074AX0"]
["6AV6371-1HV07-5AX0","WinCC/Audit RT V7.5, per operator panel, generation of an audit trail, Option for WinCC V7.5, runtime software, Single license, SW and License Key Download ******************************* E-mail address required for delivery",766,"ST",1,"SIMATIC",1E-3,1,"6AV63711HV075AX0"]
["6AV6371-1HV17-4AX0","WinCC/Audit RC V7.4, for configuration of the Audit Trail (RT and eng.) with Versioning, incl. RT license, Option for WinCC V7.4, Runtime/Configuration software, Single license, SW and License Key Download ******************************* E-mail address required for delivery",6748,"ST",1,"SIMATIC",1E-3,1,"6AV63711HV174AX0"]
["6AV6371-1HV17-5AX0","WinCC/Audit RC V7.5 for configuration of the Audit Trail (RT and eng.) with Versioning, incl. RT license, Option for WinCC V7.4, Runtime/Configuration software, Single license, SW and License Key Download ******************************* E-mail address required for delivery",6748,"ST",1,"SIMATIC",1E-3,1,"6AV63711HV175AX0"]
["6AV6371-1HV27-4AX0","WinCC/Change-Control V7.4, for configuration of the Audit Trail (English) with Versioning, incl. RT license, Option for WinCC V7.4, Runtime/Configuration software, Single license, SW and License Key Download ******************************* E-mail address required for delivery",4499,"ST",1,"SIMATIC",1E-3,1,"6AV63711HV274AX0"]
["6AV6371-1HV27-5AX0","WinCC/Change-Control V7.5 for configuration of the Audit Trail (English) with Versioning, incl. RT license, Option for WinCC V7.4, Runtime/Configuration software, Single license, SW and License Key Download ******************************* E-mail address required for delivery",4499,"ST",1,"SIMATIC",1E-3,1,"6AV63711HV275AX0"]
["6AV6371-1KG07-4AX3","WinCC/ProAgent Upgrade from V7.X to V7.4 for SIMATIC WinCC V7.4, runtime software, Single license, SW and License Key Download ******************************* E-mail address required for delivery",175,"ST",1,"SIMATIC",1E-3,1,"6AV63711KG074AX3"]
["6AV6371-1KG07-5AX3","WinCC/ProAgent upgrade from V7.2/7.3 to V7.5 for SIMATIC WinCC V7.5, runtime software, single license, SW and license key download Please observe product release: support.industry.siemens.com SIOS entry ID:  109759995 ******************************* E-mail address required for delivery",247,"ST",1,"SIMATIC",1E-3,1,"6AV63711KG075AX3"]
["6AV6371-1KG07-5AX4","WinCC/ProAgent upgrade from V7.4 to V7.5 for SIMATIC WinCC V7.5, runtime software, single license, SW and license key download Please observe product release: support.industry.siemens.com SIOS entry ID:  109759995 ******************************* E-mail address required for delivery",175,"ST",1,"SIMATIC",1E-3,1,"6AV63711KG075AX4"]
["6AV6371-1KV07-4BX3","WinCC/Audit RT Upgrade from V7.X to V7.4 for WinCC/Audit RT, runtime software, Single license, SW and License Key Download ******************************* E-mail address required for delivery",170,"ST",1,"SIMATIC",1E-3,1,"6AV63711KV074BX3"]
["6AV6371-1KV07-5BX3","WinCC/Audit RT Upgrade from V7.2/7.3 to V7.5 for WinCC/Audit RT, runtime software, Single license, SW and License Key Download ******************************* E-mail address required for delivery",170,"ST",1,"SIMATIC",1E-3,1,"6AV63711KV075BX3"]
["6AV6371-1KV07-5BX4","WinCC/Audit RT Upgrade from V7.4 to V7.5 for WinCC/Audit RT, runtime software, Single license, SW and License Key Download ******************************* E-mail address required for delivery",113,"ST",1,"SIMATIC",1E-3,1,"6AV63711KV075BX4"]
["6AV6371-1KV17-4BX3","WinCC/Audit RC Upgrade from V7.X to V7.4 for WinCC/Audit RC, and WinCC/Change-Control, Runtime/Configuration software, Single license, SW and License Key Download ******************************* E-mail address required for delivery",844,"ST",1,"SIMATIC",1E-3,1,"6AV63711KV174BX3"]
["6AV6371-1KV17-5BX3","SIMATIC WinCC/Audit RC Upgrade V7.2/7.3 to V7.5 for WinCC/Audit RC, and WinCC/Change-Control, Runtime/Configuration software, Single license, SW and License Key Download ******************************* E-mail address required for delivery",844,"ST",1,"SIMATIC",1E-3,1,"6AV63711KV175BX3"]
["6AV6371-1KV17-5BX4","SIMATIC WinCC/Audit RC Upgrade V7.4 to V7.5 for WinCC/Audit RC, and WinCC/Change-Control, Runtime/Configuration software, Single license, SW and License Key Download ******************************* E-mail address required for delivery",562,"ST",1,"SIMATIC",1E-3,1,"6AV63711KV175BX4"]
["6AV6371-2BD07-4AJ0","WinCC Power Pack RT 128/512 for WinCC V7.4, Runtime license without version change from 128 to 512 PowerTags, Single license, License key download ******************************* E-mail address required for delivery",1277,"ST",1,"SIMATIC",1E-3,1,"6AV63712BD074AJ0"]
["6AV6371-2BD07-4AX0","WinCC Powerpack RT 128/512 for WinCC V7.4, Runtime license without version change from 128 to 512 PowerTags, single license, License key on USB flash drive ******************************* Content: 1x USB",1437,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BD074AX0"]
["6AV6371-2BD07-5AJ0","WinCC Powerpack RT 128/512 for WinCC V7.5, runtime license without version change from 128 to 512 power tags, Single license, license key download ******************************* E-mail address required for delivery",1277,"ST",1,"SIMATIC",1E-3,1,"6AV63712BD075AJ0"]
["6AV6371-2BD07-5AX0","WinCC Powerpack RT 128/512 for WinCC V7.5, Runtime license without version change from 128 to 512 PowerTags, single license, License key on USB flash drive ******************************* Content: 1x USB",1437,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BD075AX0"]
["6AV6371-2BD17-4AJ0","WinCC Power Pack RC 128/512 for WinCC V7.4, RT+CS license without version change from 128 to 512 PowerTags, floating license License key download ******************************* E-mail address required for delivery",2509,"ST",1,"SIMATIC",1E-3,1,"6AV63712BD174AJ0"]
["6AV6371-2BD17-4AX0","WinCC Powerpack RC 128/512 for WinCC V7.4, RT+CS license without version change from 128 to 512 PowerTags, Floating License, License key on USB flash drive ******************************* Content: 1x USB",2821,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BD174AX0"]
["6AV6371-2BD17-5AJ0","WinCC Powerpack RC 128/512 for WinCC V7.5, runtime/configuration license without version change from 128 to 512 power tags, floating license, license key download ******************************* E-mail address required for delivery",2509,"ST",1,"SIMATIC",1E-3,1,"6AV63712BD175AJ0"]
["6AV6371-2BD17-5AX0","WinCC Powerpack RC 128/512 for WinCC V7.5, runtime/configuration license without version change from 128 to 512 PowerTags, Floating License, License key on USB flash drive ******************************* Content: 1x USB",2822,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BD175AX0"]
["6AV6371-2BG07-4AJ0","WinCC Power Pack RT 512/2048 for WinCC V7.4, Runtime license without version change from 512 to 2048 PowerTags, Single license, License key download ******************************* E-mail address required for delivery",838,"ST",1,"SIMATIC",1E-3,1,"6AV63712BG074AJ0"]
["6AV6371-2BG07-4AX0","WinCC Powerpack RT 512/2048 for WinCC V7.4, Runtime license without version change from 512 to 2048 PowerTags, single license, License key on USB flash drive ******************************* Content: 1x USB",943,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BG074AX0"]
["6AV6371-2BG07-5AJ0","WinCC Powerpack RT 512/2048 for WinCC V7.5, runtime license without version change from 512 to 2048 power tags, Single license, license key download ******************************* E-mail address required for delivery",838,"ST",1,"SIMATIC",1E-3,1,"6AV63712BG075AJ0"]
["6AV6371-2BG07-5AX0","WinCC Powerpack RT 512/2048 for WinCC V7.5, Runtime license without version change from 512 to 2048 PowerTags, single license, License key on USB flash drive ******************************* Content: 1x USB",943,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BG075AX0"]
["6AV6371-2BG17-4AJ0","WinCC Power Pack RC 512/2048 for WinCC V7.4, RT+CS license without version change from 512 to 2048 PowerTags, floating license License key download ******************************* E-mail address required for delivery",1743,"ST",1,"SIMATIC",1E-3,1,"6AV63712BG174AJ0"]
["6AV6371-2BG17-4AX0","WinCC Powerpack RC 512/2048 for WinCC V7.4, RT+CS license without version change from 512 to 2048 PowerTags, Floating License, License key on USB flash drive ******************************* Content: 1x USB",1961,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BG174AX0"]
["6AV6371-2BG17-5AJ0","WinCC Powerpack RC 512/2048 for WinCC V7.5, runtime/configuration license without version change from 512 to 2048 power tags, floating license, license key download ******************************* E-mail address required for delivery",1743,"ST",1,"SIMATIC",1E-3,1,"6AV63712BG175AJ0"]
["6AV6371-2BG17-5AX0","WinCC Powerpack RC 512/2048 for WinCC V7.5, runtime/configuration license without version change from 512 to 2048 PowerTags, Floating License, License key on USB flash drive ******************************* Content: 1x USB",1962,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BG175AX0"]
["6AV6371-2BM07-4AJ0","WinCC Power Pack RT 2048/8192 for WinCC V7.4, Runtime license without version change from 2048 to 8192 PowerTags, Single license, License key download ******************************* E-mail address required for delivery",906,"ST",1,"SIMATIC",1E-3,1,"6AV63712BM074AJ0"]
["6AV6371-2BM07-4AX0","WinCC Powerpack RT 2048/8192 for WinCC V7.4, Runtime license without version change from 2048 to 8192 PowerTags, single license, License key on USB flash drive ******************************* Content: 1x USB",1018,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BM074AX0"]
["6AV6371-2BM07-5AJ0","WinCC Powerpack RT 2048/8192 for WinCC V7.5, runtime license without version change from 2048 to 8192 power tags, Single license, license key download ******************************* E-mail address required for delivery",906,"ST",1,"SIMATIC",1E-3,1,"6AV63712BM075AJ0"]
["6AV6371-2BM07-5AX0","WinCC Powerpack RT 2048/8192 for WinCC V7.5, Runtime license without version change from 2048 to 8192 PowerTags, single license, License key on USB flash drive ******************************* Content: 1x USB",1019,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BM075AX0"]
["6AV6371-2BM17-4AJ0","WinCC Power Pack RC 2048/8192 for WinCC V7.4, RT+CS license without version change from 2048 to 8192 PowerTags, floating license License key download ******************************* E-mail address required for delivery",1856,"ST",1,"SIMATIC",1E-3,1,"6AV63712BM174AJ0"]
["6AV6371-2BM17-4AX0","WinCC Powerpack RC 2048/8192 for WinCC V7.4, RT+CS license without version change from 2048 to 8192 PowerTags, Floating License, License key on USB flash drive ******************************* Content: 1x USB",2087,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BM174AX0"]
["6AV6371-2BM17-5AJ0","WinCC Powerpack RC 2048/8192 for WinCC V7.5, runtime/configuration license without version change from 2048 to 8192 power tags, floating license, license key download ******************************* E-mail address required for delivery",1856,"ST",1,"SIMATIC",1E-3,1,"6AV63712BM175AJ0"]
["6AV6371-2BM17-5AX0","WinCC Powerpack RC 2048/8192 for WinCC V7.5, runtime/configuration license without version change from 2048 to 8192 PowerTags, Floating License, License key on USB flash drive ******************************* Content: 1x USB",2087,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BM175AX0"]
["6AV6371-2BN07-4AJ0","WinCC Power Pack RT 8192/65536 for WinCC V7.4, Runtime license without version change from 8192 to 65536 PowerTags, Single license, License key download ******************************* E-mail address required for delivery",1237,"ST",1,"SIMATIC",1E-3,1,"6AV63712BN074AJ0"]
["6AV6371-2BN07-4AX0","WinCC Powerpack RT 8192/65536 for WinCC V7.4, Runtime license without version change from 8192 to 65536 PowerTags, single license, License key on USB flash drive ******************************* Content: 1x USB",1392,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BN074AX0"]
["6AV6371-2BN07-5AJ0","WinCC Powerpack RT 8192/65536 for WinCC V7.5, runtime license without version change from 8192 to 65536 power tags, Single license, license key download ******************************* E-mail address required for delivery",1237,"ST",1,"SIMATIC",1E-3,1,"6AV63712BN075AJ0"]
["6AV6371-2BN07-5AX0","WinCC Powerpack RT 8192/65536 for WinCC V7.5, Runtime license without version change from 8192 to 65536 PowerTags, single license, License key on USB flash drive ******************************* Content: 1x USB",1392,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BN075AX0"]
["6AV6371-2BN17-4AJ0","WinCC Power Pack RC 8192/65536 for WinCC V7.4, RT+CS license without version change from 8192 to 65536 PowerTags, floating license License key download ******************************* E-mail address required for delivery",1574,"ST",1,"SIMATIC",1E-3,1,"6AV63712BN174AJ0"]
["6AV6371-2BN17-4AX0","WinCC Powerpack RC 8192/65536 for WinCC V7.4, RT+CS license without version change from 8192 to 65536 PowerTags, Floating License, License key on USB flash drive ******************************* Content: 1x USB",1771,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BN174AX0"]
["6AV6371-2BN17-5AJ0","WinCC Powerpack RC 8192/65536 for WinCC V7.5, runtime/configuration license without version change from 8192 to 65536 power tags, floating license, license key download ******************************* E-mail address required for delivery",1574,"ST",1,"SIMATIC",1E-3,1,"6AV63712BN175AJ0"]
["6AV6371-2BN17-5AX0","WinCC Powerpack RC 8192/65536 for WinCC V7.5, runtime/configuration license without version change from 8192 to 65536 PowerTags, Floating License, License key on USB flash drive ******************************* Content: 1x USB",1771,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BN175AX0"]
["6AV6371-2BP07-4AJ0","WinCC Power Pack RT 65536/102400 for WinCC V7.4, Runtime license without version change from 65536 to 102400 PowerTags, Single license, License key download ******************************* E-mail address required for delivery",2699,"ST",1,"SIMATIC",1E-3,1,"6AV63712BP074AJ0"]
["6AV6371-2BP07-4AX0","WinCC Powerpack RT 65536/102400 for WinCC V7.4, Runtime license without version change from 65536 to 102400 PowerTags, single license, License key on USB flash drive ******************************* Content: 1x USB",3036,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BP074AX0"]
["6AV6371-2BP07-5AJ0","WinCC Powerpack RT 65536/102400 for WinCC V7.5, runtime license without version change from 65536 to 102400 power tags, single license, license key download ******************************* E-mail address required for delivery",2699,"ST",1,"SIMATIC",1E-3,1,"6AV63712BP075AJ0"]
["6AV6371-2BP07-5AX0","WinCC Powerpack RT 65536/102400 for WinCC V7.5, Runtime license without version change from 65536 to 102400 PowerTags, single license, License key on USB flash drive ******************************* Content: 1x USB",3036,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BP075AX0"]
["6AV6371-2BP17-4AJ0","WinCC Power Pack RC 65536/102400 for WinCC V7.4, RT+CS license without version change from 65536 to 102400 PowerTags, floating license License key download ******************************* E-mail address required for delivery",911,"ST",1,"SIMATIC",1E-3,1,"6AV63712BP174AJ0"]
["6AV6371-2BP17-4AX0","WinCC Powerpack RC 65536/102400 for WinCC V7.4, RT+CS license without version change from 65536 to 102400 PowerTags, Floating License, License key on USB flash drive ******************************* Content: 1x USB",1024,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BP174AX0"]
["6AV6371-2BP17-5AJ0","WinCC Powerpack RC 65536/102400 for WinCC V7.5, runtime/configuration license without version change from 65536 to 102400 power tags, floating license, license key download ******************************* E-mail address required for delivery",911,"ST",1,"SIMATIC",1E-3,1,"6AV63712BP175AJ0"]
["6AV6371-2BP17-5AX0","WinCC Powerpack RC 65536/102400 for WinCC V7.5, runtime/configuration license without version change from 65536 to 102400 PowerTags, Floating License, License key on USB flash drive ******************************* Content: 1x USB",1024,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BP175AX0"]
["6AV6371-2BQ07-4AJ0","WinCC Powerp. RT 102400/153600 for WinCC V7.4, Runtime license without version change from 102400 to 153600 PowerTags, Single license, License key download ******************************* E-mail address required for delivery",2812,"ST",1,"SIMATIC",1E-3,1,"6AV63712BQ074AJ0"]
["6AV6371-2BQ07-4AX0","WinCC Powerp. RT 102400/153600 for WinCC V7.4, Runtime license without version change from 102400 to 153600 PowerTags, single license, License key on USB flash drive ******************************* Content: 1x USB",3163,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BQ074AX0"]
["6AV6371-2BQ07-5AJ0","WinCC Powerp. RT 102400/153600 for WinCC V7.5, runtime license without version change from 102400 to 153600 power tags, single license, license key download ******************************* E-mail address required for delivery",2812,"ST",1,"SIMATIC",1E-3,1,"6AV63712BQ075AJ0"]
["6AV6371-2BQ07-5AX0","WinCC Powerp. RT 102400/153600 for WinCC V7.5, Runtime license without version change from 102400 to 153600 PowerTags, single license, License key on USB flash drive ******************************* Content: 1x USB",3163,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BQ075AX0"]
["6AV6371-2BQ17-4AJ0","WinCC Powerp. RC 102400/153600 for WinCC V7.4, RT+CS license without version change from 102400 to 153600 PowerTags, floating license License key download ******************************* E-mail address required for delivery",788,"ST",1,"SIMATIC",1E-3,1,"6AV63712BQ174AJ0"]
["6AV6371-2BQ17-4AX0","WinCC Powerp. RC 102400/153600 for WinCC V7.4, RT+CS license without version change from 102400 to 153600 PowerTags, Floating License, License key on USB flash drive ******************************* Content: 1x USB",887,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BQ174AX0"]
["6AV6371-2BQ17-5AJ0","WinCC Powerp. RC 102400/153600 for WinCC V7.5, runtime/configuration license without version change from 102400 to 153600 power tags, floating license, license key download ******************************* E-mail address required for delivery",788,"ST",1,"SIMATIC",1E-3,1,"6AV63712BQ175AJ0"]
["6AV6371-2BQ17-5AX0","WinCC Powerp. RC 102400/153600 for WinCC V7.5, runtime/configuration license without version change from 102400 to 153600 PowerTags, Floating License, License key on USB flash drive ******************************* Content: 1x USB",888,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BQ175AX0"]
["6AV6371-2BR07-4AJ0","WinCC Powerp. RT 153600/262144 for WinCC V7.4, Runtime license without version change from 153600 to 262144 PowerTags, Single license, License key download ******************************* E-mail address required for delivery",4499,"ST",1,"SIMATIC",1E-3,1,"6AV63712BR074AJ0"]
["6AV6371-2BR07-4AX0","WinCC Powerp. RT 153600/262144 for WinCC V7.4, Runtime license without version change from 153600 to 262144 PowerTags, single license, License key on USB flash drive ******************************* Content: 1x USB",5058,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BR074AX0"]
["6AV6371-2BR07-5AJ0","WinCC Powerp. RT 153600/262144 for WinCC V7.5, runtime license without version change from 153600 to 262144 power tags, single license, license key download ******************************* E-mail address required for delivery",4499,"ST",1,"SIMATIC",1E-3,1,"6AV63712BR075AJ0"]
["6AV6371-2BR07-5AX0","WinCC Powerp. RT 153600/262144 for WinCC V7.5, Runtime license without version change from 153600 to 262144 PowerTags, single license, License key on USB flash drive ******************************* Content: 1x USB",5058,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BR075AX0"]
["6AV6371-2BR17-4AJ0","WinCC Powerp. RC 153600/262144 for WinCC V7.4, RT+CS license without version change from 153600 to 262144 PowerTags, floating license License key download ******************************* E-mail address required for delivery",4162,"ST",1,"SIMATIC",1E-3,1,"6AV63712BR174AJ0"]
["6AV6371-2BR17-4AX0","WinCC Powerp. RC 153600/262144 for WinCC V7.4, RT+CS license without version change from 153600 to 262144 PowerTags, Floating License, License key on USB flash drive ******************************* Content: 1x USB",4679,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BR174AX0"]
["6AV6371-2BR17-5AJ0","WinCC Powerp. RC 153600/262144 for WinCC V7.5, runtime/configuration license without version change from 153600 to 262144 power tags, floating license, license key download ******************************* E-mail address required for delivery",4162,"ST",1,"SIMATIC",1E-3,1,"6AV63712BR175AJ0"]
["6AV6371-2BR17-5AX0","WinCC Powerp. RC 153600/262144 for WinCC V7.5, runtime/configuration license without version change from 153600 to 262144 PowerTags, Floating License, License key on USB flash drive ******************************* Content: 1x USB",4680,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63712BR175AX0"]
["6AV6372-1DC07-4AX0","WinCC/Calendar Scheduler V7.4, Option for WinCC V7.4 Runtime/configuration software on CD-ROM, single license, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",949,"ST",1,"SIMATIC",0.17100000000000001,1,"6AV63721DC074AX0"]
["6AV6372-1DC07-4AX3","WinCC/Calendar Options Upgrade from V7.X to V7.4 for WinCC Options WinCC/Calendar Scheduler and WinCC/Event Notifier, Runtime/configuration software on CD-ROM, single license, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",208,"ST",1,"SIMATIC",0.17100000000000001,1,"6AV63721DC074AX3"]
["6AV6372-1DC07-5AX0","WinCC/Calendar Scheduler V7.5, option for WinCC V7.5 Runtime/configuration software on CD-ROM, single license, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",950,"ST",1,"SIMATIC",0.19800000000000001,1,"6AV63721DC075AX0"]
["6AV6372-1DC07-5AX3","WinCC/Calendar Options Upgrade from V7.2/7.3 to V7.5 for WinCC Options WinCC/Calendar Scheduler and WinCC/Event Notifier, Runtime/configuration software on CD-ROM, single license, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",208,"ST",1,"SIMATIC",0.19800000000000001,1,"6AV63721DC075AX3"]
["6AV6372-1DC07-5AX4","WinCC/Calendar Options Upgrade from V7.4 to V7.5 for WinCC Options WinCC/Calendar Scheduler and WinCC/Event Notifier, Runtime/configuration software on CD-ROM, single license, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",139,"ST",1,"SIMATIC",0.19800000000000001,1,"6AV63721DC075AX4"]
["6AV6372-1DD07-4AX0","WinCC/Event Notifier V7.4, Option for WinCC V7.4, Runtime/configuration software on CD-ROM, single license, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",1897,"ST",1,"SIMATIC",0.17100000000000001,1,"6AV63721DD074AX0"]
["6AV6372-1DD07-5AX0","WinCC/Event Notifier V7.5, Option for WinCC V7.5, Runtime/configuration software on CD-ROM, single license, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",1898,"ST",1,"SIMATIC",0.19800000000000001,1,"6AV63721DD075AX0"]
["6AV6372-1DE04-0AX0","SIMATIC powerrate V4.0 SP3 Engineering+AS-RT (unlimited), Power Management for WinCC V7.4/V7.3 Second Edition/ V7.2, PCS 7 V8.1 SP1/V8.1/ V8.0 SP2/V7.1 SP4; ES/R-SW, single license SW and documentation on DVD, License key on USB stick, Class A, 2 languages (de, en)",4055,"ST",1,"SIMATIC",0.27700000000000002,1,"6AV63721DE040AX0"]
["6AV6372-1DE04-0AX3","SIMATIC powerrate V4.0 SP3 Engineering+AS-RT (unlimited), Update V4.0 (SP1)-> V4.0 SP3 Data carrier without license, Use only in connection with a valid license, Power Management for WinCC V7.4/V7.3 Second Edition/ V7.2, PCS 7 V8.1 SP1/V8.1/ V8.0 SP2/V7.1 SP4; SW and documentation on DVD",58,"ST",1,"SIMATIC",0.26700000000000002,1,"6AV63721DE040AX3"]
["6AV6372-1DE04-0AX4","SIMATIC powerrate V4.0 SP3 Engineering+AS-RT (unlimited), Upgrade V3.X-> V4.0 SP3, Power Management for WinCC V7.4/V7.3 Second Edition/ V7.2, PCS 7 V8.1 SP1/V8.1/ V8.0 SP2/V7.1 SP4; ES/R-SW, Single license, SW and documentation on DVD, License key on USB stick, Class A, 2 languages (de, en)",1042,"ST",1,"SIMATIC",0.27700000000000002,1,"6AV63721DE040AX4"]
["6AV6372-1DE04-0AX7","SIMATIC powerrate V4.0 SP3 Trial (30 days), Power Management for WinCC V7.4/V7.3 Second Edition/ V7.2, PCS 7 V8.1 SP1/V8.1/ V8.0 SP2/V7.1 SP4; SW and documentation on DVD, 2 languages (de, en)",58,"ST",1,"SIMATIC",0.183,1,"6AV63721DE040AX7"]
["6AV6372-1DF07-1AH0","SIMATIC Energy Manager Basic V7.1; including 50 tags, 1 data acquisition component, 1 web client; Engineering/Runtime software; Single license software, documentation and License key for download; 6 languages: de,en,fr,es,it,zh; executable on (64-bit) Windows 7 Pro/Ultimate, Windows 8.1 Pro/Enterprise, Windows 10 Pro/Enterprise, Windows Server 2008 R2, 2012 R2, Windows Server 2016 ******************************* E-mail address required for delivery",3150,"ST",1,"SIMATIC",1E-3,1,"6AV63721DF071AH0"]
["6AV6372-1DF07-1AX0","SIMATIC Energy Manager Basic V7.1; including 50 tags, 1 data acquisition component, 1 web client; Engineering/Runtime software; Single License; license key on USB stick; Software and documentation on DVD; 6 languages: de,en,fr,es,it,zh; executable on (64 bit) Windows 7 Pro/Ultimate, Windows 8.1 Pro/Enterprise, Windows 10 Pro/Enterprise, Windows Srv 2008 R2, 2012 R2, Windows Srv 2016 ******************************* Content: Set (1x DVD + 1x USB)",3213,"ST",1,"SIMATIC",0.19400000000000001,1,"6AV63721DF071AX0"]
["6AV6372-1HC07-4AX0","WinCC/Calendar Scheduler V7.4, Option for WinCC V7.4 Runtime/Configuration software Single license, SW and License Key Download ******************************* E-mail address required for delivery",844,"ST",1,"SIMATIC",1E-3,1,"6AV63721HC074AX0"]
["6AV6372-1HC07-5AX0","WinCC/Calendar Scheduler V7.5, Option for WinCC V7.5 Runtime/Configuration software Single license, SW and License Key Download ******************************* E-mail address required for delivery",844,"ST",1,"SIMATIC",1E-3,1,"6AV63721HC075AX0"]
["6AV6372-1HD07-4AX0","WinCC/Event Notifier V7.4, Option for WinCC V7.4, Runtime/Configuration software Single license, SW and License Key Download ******************************* E-mail address required for delivery",1688,"ST",1,"SIMATIC",1E-3,1,"6AV63721HD074AX0"]
["6AV6372-1HD07-5AX0","WinCC/Event Notifier V7.5, Option for WinCC V7.5, Runtime/Configuration software Single license, SW and License Key Download ******************************* E-mail address required for delivery",1688,"ST",1,"SIMATIC",1E-3,1,"6AV63721HD075AX0"]
["6AV6372-1KC07-4AX3","WinCC/Calendar Options Upgrade from V7.X to V7.4 for WinCC Options WinCC/Calendar Scheduler and WinCC/Event Notifier, Runtime/Configuration software Single license, SW and License Key Download ******************************* E-mail address required for delivery",185,"ST",1,"SIMATIC",1E-3,1,"6AV63721KC074AX3"]
["6AV6372-1KC07-5AX3","WinCC/Calendar Options Upgrade from V7.2/7.3 to V7.5 for WinCC Options WinCC/Calendar Scheduler and WinCC/Event Notifier, Runtime/Configuration software Single license, SW and License Key Download ******************************* E-mail address required for delivery",185,"ST",1,"SIMATIC",1E-3,1,"6AV63721KC075AX3"]
["6AV6372-1KC07-5AX4","WinCC/Calendar Options Upgrade from V7.4 to V7.5 for WinCC Options WinCC/Calendar Scheduler and WinCC/Event Notifier, Runtime/Configuration software Single license, SW and License Key Download ******************************* E-mail address required for delivery",123,"ST",1,"SIMATIC",1E-3,1,"6AV63721KC075AX4"]
["6AV6372-2BJ07-4BA0","Sequence execution system, Extension by 5 units, for SIMATIC WinCC V7.4, Runtime software, single license, count relevant, License key on USB flash drive ******************************* Content: 1x USB",1241,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722BJ074BA0"]
["6AV6372-2BJ07-5BA0","Sequence Execution System, extension 5 units, for SIMATIC WinCC V7.5, Runtime software, single license, count relevant, License key on USB flash drive ******************************* Content: 1x USB",1242,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722BJ075BA0"]
["6AV6372-2BJ17-4BA0","Sequence execution system, extension 5 units upgrade, for SIMATIC WinCC V7.4, Runtime software, single license, count relevant, License key on USB flash drive ******************************* Content: 1x USB",620,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722BJ174BA0"]
["6AV6372-2BJ17-5BA0","Sequence Execution System, extension 5 units upgrade, for SIMATIC WinCC V7.5, Runtime software, single license, count relevant, License key on USB flash drive ******************************* Content: 1x USB",625,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722BJ175BA0"]
["6AV6372-2BJ17-5BA1","Sequence Execution System, extension 5 units upgrade, for SIMATIC WinCC V7.5, Runtime software, single license, count relevant, License key on USB flash drive ******************************* Content: 1x USB",413,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722BJ175BA1"]
["6AV6372-2CG20-0BA0","WinCC/Performance Mon. Arch., 30 archive variables, for WinCC V7.2 or higher, runtime software, single license, count relevant, License key on USB flash drive ******************************* Content: 1x USB",1116,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722CG200BA0"]
["6AV6372-2CG20-0CA0","WinCC/Performance Mon. Arch., 100 archive variables, for WinCC V7.2 or higher, runtime software, single license, count relevant, License key on USB flash drive ******************************* Content: 1x USB",3349,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722CG200CA0"]
["6AV6372-2CG20-0DA0","WinCC/Performance Mon. Arch., 300 archive variables, for WinCC V7.2 or higher, runtime software, single license, count relevant, License key on USB flash drive ******************************* Content: 1x USB",9040,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722CG200DA0"]
["6AV6372-2CG20-0EA0","WinCC/Performance Mon. Arch., 1000 archive variables, for WinCC V7.2 or higher, runtime software, single license, count relevant, License key on USB flash drive ******************************* Content: 1x USB",30129,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722CG200EA0"]
["6AV6372-2DF00-0CL0","SIMATIC EnergyManager Basic/PRO for up to 50 Tags, 1 Consumer Software Update Service, within the framework of this contract, you will receive for one year all up-to-date software versions, the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software",1286,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV63722DF000CL0"]
["6AV6372-2DF00-0CY0","SIMATIC EnergyManager Basic/PRO for < 50 Tags, 1 Consumer Software Update Service; within the framework of this contract, you will receive for one year all up-to-date software versions, the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice. Requirement for conclusion: current version of the software ******************************* e-mail address required for delivery",1260,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF000CY0"]
["6AV6372-2DF00-0DL0","SIMATIC Energy Manager PRO for systems with up to 100 tags, Software Update Service, within the framework of this contract, you will receive for one year all up-to-date software versions, the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software",1928,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV63722DF000DL0"]
["6AV6372-2DF00-0DY0","SIMATIC Energy Manager PRO for systems with up to 100 tags, Software Update Service; within the framework of this contract, you will receive for one year all up-to-date software versions, the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice. Requirement for conclusion: current version of the software ******************************* e-mail address required for delivery",1890,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF000DY0"]
["6AV6372-2DF00-0FL0","SIMATIC Energy Manager PRO for systems with up to 500 tags, Software Update Service within the framework of this contract, you will receive for one year all up-to-date software versions, the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software",3856,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV63722DF000FL0"]
["6AV6372-2DF00-0FY0","SIMATIC Energy Manager PRO for systems with up to 500 tags, Software Update Service; within the framework of this contract, you will receive for one year all up-to-date software versions, the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice. Requirement for conclusion: current version of the software ******************************* e-mail address required for delivery",3780,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF000FY0"]
["6AV6372-2DF00-0HL0","SIMATIC Energy Manager PRO for systems with up to 5000 tags, Software Update Service within the framework of this contract, you will receive for one year all up-to-date software versions, the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software",6426,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV63722DF000HL0"]
["6AV6372-2DF00-0HY0","SIMATIC Energy Manager PRO for systems with up to 5000 tags, Software Update Service; within the framework of this contract, you will receive for one year all up-to-date software versions, the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice. Requirement for conclusion: current version of the software ******************************* e-mail address required for delivery",6300,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF000HY0"]
["6AV6372-2DF07-0CH0","SIMATIC Energy Manager Basic/PRO Tag Package 50; increases the number of tags by 50 tags; Engineering/Runtime software; Single License; License key for download; Without software and documentation ******************************* e-mail address required for delivery",4200,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF070CH0"]
["6AV6372-2DF07-0CX0","SIMATIC Energy Manager Basic/PRO Tag Package 50; increases the number of tags by 50 tags; Engineering/Runtime software; Single License; license key on USB stick; without software and documentation ******************************* Content: 1x USB",4284,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722DF070CX0"]
["6AV6372-2DF07-0DH0","SIMATIC Energy Manager Basic/PRO Tag Package 100; increases the number of tags by 100 tags; Engineering/Runtime software; Single License; License key for download; without software and documentation ******************************* e-mail address required for delivery",7350,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF070DH0"]
["6AV6372-2DF07-0DX0","SIMATIC Energy Manager Basic/PRO Tag Package 100; increases the number of tags by 100 tags; Engineering/Runtime software; Single License; license key on USB stick; without software and documentation ******************************* Content: 1x USB",7497,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722DF070DX0"]
["6AV6372-2DF07-0EH0","SIMATIC Energy Manager Basic/PRO Tag Package 250; increases the number of tags by 250 tags; Engineering/Runtime software; Single License; License key for download; without software and documentation ******************************* e-mail address required for delivery",10500,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF070EH0"]
["6AV6372-2DF07-0EX0","SIMATIC Energy Manager Basic/PRO Tag Package 250; increases the number of tags by 250 tags; Engineering/Runtime software; Single License; license key on USB stick; without software and documentation ******************************* Content: 1x USB",10710,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722DF070EX0"]
["6AV6372-2DF07-0FH0","SIMATIC Energy Manager Basic/PRO Tag Package 500; increases the number of tags by 500 tags; Engineering/Runtime software; Single License; License key for download; without software and documentation ******************************* e-mail address required for delivery",14700,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF070FH0"]
["6AV6372-2DF07-0FX0","SIMATIC Energy Manager Basic/PRO Tag Package 500; increases the number of tags by 500 tags; Engineering/Runtime software; Single License; license key on USB stick; without software and documentation ******************************* Content: 1x USB",14994,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722DF070FX0"]
["6AV6372-2DF07-0GH0","SIMATIC Energy Manager Basic/PRO Tag Package 1000; increases the number of tags by 1000 tags; Engineering/Runtime software; Single License; License key for download; without software and documentation ******************************* e-mail address required for delivery",25200,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF070GH0"]
["6AV6372-2DF07-0GX0","SIMATIC Energy Manager Basic/PRO Tag Package 1000; increases the number of tags by 1000 tags; Engineering/Runtime software; Single License; license key on USB stick; without software and documentation ******************************* Content: 1x USB",25704,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722DF070GX0"]
["6AV6372-2DF07-0HH0","SIMATIC Energy Manager Basic/PRO Tag Package 5000; increases the number of tags by 5000 tags; Engineering/Runtime software; Single License; License key for download; without software and documentation ******************************* e-mail address required for delivery",29400,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF070HH0"]
["6AV6372-2DF07-0HX0","SIMATIC Energy Manager Basic/PRO Tag Package 5000; increases the number of tags by 5000 tags; Engineering/Runtime software; Single License; license key on USB stick; without software and documentation ******************************* Content: 1x USB",29988,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722DF070HX0"]
["6AV6372-2DF07-0JH0","SIMATIC Energy Manager Basic/PRO Tag Package 30000; increases the number of tags by 30000 tags; Engineering/Runtime software; Single License; License key for download; without software and documentation ******************************* e-mail address required for delivery",35700,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF070JH0"]
["6AV6372-2DF07-0JX0","SIMATIC Energy Manager Basic/PRO Tag Package 30000; increases the number of tags by 30000 tags; Engineering/Runtime software; Single License; license key on USB stick; without software and documentation ******************************* Content: 1x USB",36414,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722DF070JX0"]
["6AV6372-2DF07-1AH0","SIMATIC Energy Manager PRO V7.1; including 50 tags, 1 data acquisition component, 1 client, 1 web client; Engineering/Runtime software; Single license software, documentation and License key for download; 2 languages: de,en; Web client 6 languages: de,en,it,es,fr,zh; executable on (64-bit) Windows 7 Pro/Ultimate, Windows 8.1 Pro/Enterprise, Windows 10 Pro/Enterprise, Windows Server 2008 R2, 2012 R2, Windows Server 2016 ******************************* E-mail address required for delivery",6300,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF071AH0"]
["6AV6372-2DF07-1AH3","SIMATIC Energy Manager PRO V7.1, Power Pack for upgrade from Energy Manager Basic V7.1 to Energy Manager PRO V7.1; including 1 client, Engineering/Runtime software; Single license License key for download; without software and documentation ******************************* E-mail address required for delivery",3150,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF071AH3"]
["6AV6372-2DF07-1AL2","Siemens Solution Partner, Partner contribution for Specialist Program Module \"Industrial Energy Management\" annual contribution",840,"ST",1,"SIMATIC",0.56699999999999995,1,"6AV63722DF071AL2"]
["6AV6372-2DF07-1AX0","SIMATIC Energy Manager PRO V7.1; including 50 tags, 1 data acquisition component, 1 client, 1 web client; Engineering/Runtime software; Single License; license key on USB stick; Software and documentation on DVD; 2 languages: de,en; Web client 6 languages: de,en,it,es,fr,zh; executable on (64 bit) Windows 7 Pro/Ultimate, Windows 8.1 Pro/Enterprise, Windows 10 Pro/Enterprise, Windows Srv 2008 R2, 2012 R2, Windows Srv 2016 ******************************* Content: Set (1x DVD + 1x USB)",6426,"ST",1,"SIMATIC",0.19400000000000001,1,"6AV63722DF071AX0"]
["6AV6372-2DF07-1AX3","SIMATIC Energy Manager PRO V7.1, Power Pack for upgrade from Energy Manager Basic V7.1 to Energy Manager PRO V7.1; including 1 client; Engineering/Runtime software; Single License; license key on USB stick; without software and documentation ******************************* Content: 1x USB",3213,"ST",1,"SIMATIC",0.193,1,"6AV63722DF071AX3"]
["6AV6372-2DF07-1CH4","SIMATIC Energy Manager PRO Upgrade V7.0 -> V7.1 for systems with up to 50 tags, Engineering/Runtime software; Single license software, documentation and License key for download; executable on Windows 7 Pro/Ultimate, Windows 8.1 Pro/Enterprise, Windows 10 Pro/Enterprise, Windows Server 2008 R2, 2012 R2, Windows Server 2016 ******************************* E-mail address required for delivery",2520,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF071CH4"]
["6AV6372-2DF07-1CX4","SIMATIC Energy Manager PRO Upgrade V7.0 -> V7.1 for systems with up to 50 tags, Engineering/Runtime software; Single License; license key on USB stick; Software and documentation on DVD; executable on (64 bit) Windows 7 Pro/Ultimate, Windows 8.1 Pro/Enterprise, Windows 10 Pro/Enterprise, Windows Srv 2008 R2, 2012 R2, Windows Srv 2016 ******************************* Content: Set (1x DVD + 1x USB)",2571,"ST",1,"SIMATIC",0.193,1,"6AV63722DF071CX4"]
["6AV6372-2DF07-1DH4","SIMATIC Energy Manager PRO Upgrade V7.0 -> V7.1 for systems with up to 100 tags, Engineering/Runtime software; Single license software, documentation and License key for download; executable on Windows 7 Pro/Ultimate, Windows 8.1 Pro/Enterprise, Windows 10 Pro/Enterprise, Windows Server 2008 R2, 2012 R2, Windows Server 2016 ******************************* E-mail address required for delivery",3675,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF071DH4"]
["6AV6372-2DF07-1DX4","SIMATIC Energy Manager PRO Upgrade V7.0 -> V7.1 for systems with up to 100 tags, Engineering/Runtime software; Single License; license key on USB stick; Software and documentation on DVD; executable on (64 bit) Windows 7 Pro/Ultimate, Windows 8.1 Pro/Enterprise, Windows 10 Pro/Enterprise, Windows Srv 2008 R2, 2012 R2, Windows Srv 2016 ******************************* Content: Set (1x DVD + 1x USB)",3749,"ST",1,"SIMATIC",0.193,1,"6AV63722DF071DX4"]
["6AV6372-2DF07-1FH4","SIMATIC Energy Manager PRO Upgrade V7.0 -> V7.1 for systems with up to 500 tags, Engineering/Runtime software; Single license software, documentation and License key for download; executable on Windows 7 Pro/Ultimate, Windows 8.1 Pro/Enterprise, Windows 10 Pro/Enterprise, Windows Server 2008 R2, 2012 R2, Windows Server 2016 ******************************* E-mail address required for delivery",7350,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF071FH4"]
["6AV6372-2DF07-1FX4","SIMATIC Energy Manager PRO Upgrade V7.0 -> V7.1 for systems with up to 500 tags, Engineering/Runtime software; Single License; license key on USB stick; Software and documentation on DVD; executable on (64 bit) Windows 7 Pro/Ultimate, Windows 8.1 Pro/Enterprise, Windows 10 Pro/Enterprise, Windows Srv 2008 R2, 2012 R2, Windows Srv 2016 ******************************* Content: Set (1x DVD + 1x USB)",7497,"ST",1,"SIMATIC",0.193,1,"6AV63722DF071FX4"]
["6AV6372-2DF07-1HH4","SIMATIC Energy Manager PRO Upgrade V7.0 -> V7.1 for systems with up to 5000 tags, Engineering/Runtime software; Single license software, documentation and License key for download; executable on Windows 7 Pro/Ultimate, Windows 8.1 Pro/Enterprise, Windows 10 Pro/Enterprise, Windows Server 2008 R2, 2012 R2, Windows Server 2016 ******************************* E-mail address required for delivery",12600,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF071HH4"]
["6AV6372-2DF07-1HX4","SIMATIC Energy Manager PRO Upgrade V7.0 -> V7.1 for systems with up to 5000 tags, Engineering/Runtime software; Single License; license key on USB stick; Software and documentation on DVD; executable on (64 bit) Windows 7 Pro/Ultimate, Windows 8.1 Pro/Enterprise, Windows 10 Pro/Enterprise, Windows Srv 2008 R2, 2012 R2, Windows Srv 2016 ******************************* Content: Set (1x DVD + 1x USB)",12852,"ST",1,"SIMATIC",0.193,1,"6AV63722DF071HX4"]
["6AV6372-2DF17-1AX0","SIMATIC Energy Manager Basic/PRO V7.1 Trial (90 days), Software and documentation on DVD; executable on (64 bit) Windows 7 Pro/Ultimate, Windows 8.1 Pro/Enterprise, Windows 10 Pro/Enterprise, Windows Srv 2008 R2, 2012 R2, Windows Srv 2016 ******************************* Content: 1x DVD",53.6,"ST",1,"SIMATIC",0.183,1,"6AV63722DF171AX0"]
["6AV6372-2DF27-0AH0","SIMATIC Energy Manager Basic/PRO 3 web clients; Runtime software; Single License; License key for download; without software and documentation ******************************* e-mail address required for delivery",2100,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF270AH0"]
["6AV6372-2DF27-0AX0","SIMATIC Energy Manager Basic/PRO 3 web clients; Runtime software; Single License; license key on USB stick; without software and documentation ******************************* Content: 1x USB",2142,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722DF270AX0"]
["6AV6372-2DF27-0BH0","SIMATIC Energy Manager Basic/PRO 20 web clients; Runtime software; Single License; License key for download; without software and documentation ******************************* e-mail address required for delivery",7875,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF270BH0"]
["6AV6372-2DF27-0BX0","SIMATIC Energy Manager Basic/PRO 20 web clients; Runtime software; Single License; license key on USB stick; without software and documentation ******************************* Content: 1x USB",8033,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722DF270BX0"]
["6AV6372-2DF27-0CH0","SIMATIC Energy Manager Basic/PRO 60 web clients; Runtime software; Single License; License key for download; without software and documentation ******************************* e-mail address required for delivery",15750,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF270CH0"]
["6AV6372-2DF27-0CX0","SIMATIC Energy Manager Basic/PRO 60 web clients; Runtime software; Single License; license key on USB stick; without software and documentation ******************************* Content: 1x USB",16065,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722DF270CX0"]
["6AV6372-2DF37-0AH0","SIMATIC Energy Manager PRO Client; Engineering/Runtime software; Single License; License key for download; without software and documentation ******************************* e-mail address required for delivery",1365,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF370AH0"]
["6AV6372-2DF37-0AX0","SIMATIC Energy Manager PRO Client; Engineering/Runtime software; Single License; license key on USB stick; without software and documentation ******************************* Content: 1x USB",1393,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722DF370AX0"]
["6AV6372-2DF47-0AH0","SIMATIC Energy Manager PRO Energy forecast and planning; Engineering/Runtime software; Single License; License key for download; without software and documentation ******************************* e-mail address required for delivery",6300,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF470AH0"]
["6AV6372-2DF47-0AX0","SIMATIC Energy Manager PRO Energy forecast and planning; Engineering/Runtime software; Single License; license key on USB stick; without software and documentation ******************************* Content: 1x USB",6426,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722DF470AX0"]
["6AV6372-2DF57-0AH0","SIMATIC Energy Manager PRO Data acquisition component; Connection to WinCC, OPC, ASCII, XML, ODBC...; Engineering/Runtime software; Single License; License key for download; without software and documentation ******************************* e-mail address required for delivery",2100,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF570AH0"]
["6AV6372-2DF57-0AX0","SIMATIC Energy Manager PRO Data acquisition component; Connection to WinCC, OPC, ASCII, XML, ODBC...; Engineering/Runtime software; Single License; license key on USB stick; without software and documentation ******************************* Content: 1x USB",2142,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722DF570AX0"]
["6AV6372-2DF67-0LH0","SIMATIC Energy Manager PRO Consumer license; Engineering/Runtime software; Single License; contains license certificate for 1 consumer for download ******************************* e-mail address required for delivery",625,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF670LH0"]
["6AV6372-2DF67-0LX0","SIMATIC Energy Manager PRO Consumer license; Engineering/Runtime software; Single License; contains license certificate for 1 consumer ******************************* Content: Certificate of License",638,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV63722DF670LX0"]
["6AV6372-2DF67-1AH0","SIMATIC Energy Manager PRO Consumer Package 1; including EE-Monitor; increases the number of consumers by 1 consumer; Engineering/Runtime software; Single license License key for download; without software and documentation ******************************* E-mail address required for delivery",420,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF671AH0"]
["6AV6372-2DF67-1AX0","SIMATIC Energy Manager PRO Consumer Package 1, including EE-Monitor; increases the number of consumers by 1 consumer; Engineering/Runtime software; Single License; license key on USB stick; without software and documentation ******************************* Content: 1x USB",429,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722DF671AX0"]
["6AV6372-2DF67-1BH0","SIMATIC Energy Manager PRO Consumer Package 5; including EE-Monitor; increases the number of consumers by 5 consumers; Engineering/Runtime software; Single license License key for download; without software and documentation ******************************* E-mail address required for delivery",2100,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF671BH0"]
["6AV6372-2DF67-1BX0","SIMATIC Energy Manager PRO Consumer Package 5, including EE-Monitor; increases the number of consumers by 5 consumers; Engineering/Runtime software; Single License; license key on USB stick; without software and documentation ******************************* Content: 1x USB",2142,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722DF671BX0"]
["6AV6372-2DF67-1CH0","SIMATIC Energy Manager PRO Consumer Package 25; including EE-Monitor; increases the number of consumers by 25 consumers; Engineering/Runtime software; Single license License key for download; without software and documentation ******************************* E-mail address required for delivery",10500,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF671CH0"]
["6AV6372-2DF67-1CX0","SIMATIC Energy Manager PRO Consumer Package 25; including EE-Monitor; increases the number of consumers by 25 consumers; Engineering/Runtime software; Single License; license key on USB stick; without software and documentation ******************************* Content: 1x USB",10710,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722DF671CX0"]
["6AV6372-2DF67-1MH0","SIMATIC Energy Manager PRO V7.1 Consumer Master; including 50 tags, 1 client, 20 web clients; Engineering/Runtime software; Single license software, documentation and License key for download; 2 languages: de,en; Web client 6 languages: de,en,it,es,fr,zh; executable on (64-bit) Windows 7 Pro/Ultimate, Windows 8.1 Pro/Enterprise, Windows 10 Pro/Enterprise, Windows Server 2008 R2, 2012 R2, Windows Server 2016 ******************************* E-mail address required for delivery",6300,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF671MH0"]
["6AV6372-2DF67-1MX0","SIMATIC Energy Manager PRO V7.1 Consumer Master; including 50 tags, 1 client, 20 web clients; Engineering/Runtime software; Single License; license key on USB stick; Software and documentation on DVD; 2 languages: de,en, Web client 6 languages: de,en,it,es,fr,zh; executable on (64 bit) Windows 7 Pro/Ultimate, Windows 8.1 Pro/Enterprise, Windows 10 Pro/Enterprise, Windows Srv 2008 R2, 2012 R2, Windows Srv 2016 ******************************* Content: Set (1x DVD + 1x USB)",6426,"ST",1,"SIMATIC",0.19400000000000001,1,"6AV63722DF671MX0"]
["6AV6372-2DF70-0XL0","SIMATIC Energy Manager PRO for systems > 5000 tags, Software Update Service, within the framework of this contract, you will receive for one year all up-to-date software versions, the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software",8568,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV63722DF700XL0"]
["6AV6372-2DF70-0XY0","SIMATIC Energy Manager PRO for systems > 5000 tags, Software Update Service; within the framework of this contract, you will receive for one year all up-to-date software versions, the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice. Requirement for conclusion: current version of the software ******************************* e-mail address required for delivery",8400,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF700XY0"]
["6AV6372-2DF77-1AH0","SIMATIC Energy Manager PRO Consumer Package 1; increases the number of consumers by 1 consumer; Engineering/Runtime software; Single license License key for download; without software and documentation ******************************* E-mail address required for delivery",263,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF771AH0"]
["6AV6372-2DF77-1AX0","SIMATIC Energy Manager PRO Consumer Package 1; increases the number of consumers by 1 consumer; Engineering/Runtime software; Single License; license key on USB stick; without software and documentation ******************************* Content: 1x USB",268,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722DF771AX0"]
["6AV6372-2DF77-1BH0","SIMATIC Energy Manager PRO Consumer Package 5; increases the number of consumers by 5 consumers; Engineering/Runtime software; Single license License key for download; without software and documentation ******************************* E-mail address required for delivery",1313,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF771BH0"]
["6AV6372-2DF77-1BX0","SIMATIC Energy Manager PRO Consumer Package 5; increases the number of consumers by 5 consumers; Engineering/Runtime software; Single License; license key on USB stick; without software and documentation ******************************* Content: 1x USB",1339,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722DF771BX0"]
["6AV6372-2DF77-1CH0","SIMATIC Energy Manager PRO Consumer Package 25; increases the number of consumers by 25 consumers; Engineering/Runtime software; Single license License key for download; without software and documentation ******************************* E-mail address required for delivery",6563,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF771CH0"]
["6AV6372-2DF77-1CX0","SIMATIC Energy Manager PRO Consumer Package 25; increases the number of consumers by 25 consumers; Engineering/Runtime software; Single License; license key on USB stick; without software and documentation ******************************* Content: 1x USB",6694,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV63722DF771CX0"]
["6AV6372-2DF77-1XH4","SIMATIC Energy Manager PRO Upgrade V7.0 -> V7.1 for systems > 5000 tags, Engineering/Runtime software; Single license software, documentation and License key for download; executable on (64-bit) Windows 7 Pro/Ultimate, Windows 8.1 Pro/Enterprise, Windows 10 Pro/Enterprise, Windows Server 2008 R2, 2012 R2, Windows Server 2016 ******************************* E-mail address required for delivery",16800,"ST",1,"SIMATIC",1E-3,1,"6AV63722DF771XH4"]
["6AV6372-2DF77-1XX4","SIMATIC Energy Manager PRO Upgrade V7.0 -> V7.1 for systems > 5000 tags, Engineering/Runtime software; Single License; license key on USB stick; Software and documentation on DVD; executable on (64 bit) Windows 7 Pro/Ultimate, Windows 8.1 Pro/Enterprise, Windows 10 Pro/Enterprise, Windows Srv 2008 R2, 2012 R2, Windows Srv 2016 ******************************* Content: Set (1x DVD + 1x USB)",17136,"ST",1,"SIMATIC",0.193,1,"6AV63722DF771XX4"]
["6AV6372-2DG07-4AA0","WinCC/Performance Mon. Basic P, incl. 30 archive variables, for WinCC V7.4 SP1, Runtime SW on CD-ROM, single license, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",3039,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV63722DG074AA0"]
["6AV6372-2DG07-4AX3","WinCC/Performance Mon. Upgrade from V7.X to V7.4 SP1 for WinCC V7.4 SP1, Runtime SW on CD-ROM, single license, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",1116,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV63722DG074AX3"]
["6AV6372-2DG07-5AA0","WinCC/Performance Mon. Basic P, incl. 30 archive variables, for WinCC V7.5, Runtime SW on CD-ROM, single license, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",3040,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV63722DG075AA0"]
["6AV6372-2DG07-5AX3","WinCC/Performance Mon. Upgrade from V7.2/7.3-> V7.5 for WinCC V7.5, Runtime SW on CD-ROM, single license, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",1117,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV63722DG075AX3"]
["6AV6372-2DG07-5AX4","WinCC/Performance Mon. Upgrade from V7.4-> V7.5 for WinCC V7.5, Runtime SW on CD-ROM, single license, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",744,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV63722DG075AX4"]
["6AV6372-2DJ07-4AA0","Sequence execution system, Basic PCKG. incl. 2 units, for SIMATIC WinCC V7.4, Runtime software on CD-ROM, single license, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",1861,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV63722DJ074AA0"]
["6AV6372-2DJ07-5AA0","Sequence Execution System, basic package incl. 2 units, for SIMATIC WinCC V7.5, Runtime software on CD-ROM, single license, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",1861,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV63722DJ075AA0"]
["6AV6372-2DJ17-4AA0","Sequence execution system, Basic PCKG. upgrade, for SIMATIC WinCC V7.4, Runtime software on CD-ROM, single license, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",931,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV63722DJ174AA0"]
["6AV6372-2DJ17-5AA0","Sequence Execution System, Basic Package Upgrade, for SIMATIC WinCC V7.5, Runtime software on CD-ROM, single license, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",931,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV63722DJ175AA0"]
["6AV6372-2DJ17-5AA1","Sequence Execution System, Basic Package Upgrade, for SIMATIC WinCC V7.5, Runtime software on CD-ROM, single license, license key on USB flash drive ******************************* Content: Set (1x DVD + 1x USB)",620,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV63722DJ175AA1"]
["6AV6372-2HG07-4AA0","WinCC/Performance Mon. Basic P, incl. 30 archive tags, for WinCC V7.4, Runtime software, Single license, count relevant, License key download ******************************* E-mail address required for delivery",2702,"ST",1,"SIMATIC",1E-3,1,"6AV63722HG074AA0"]
["6AV6372-2HG07-5AA0","WinCC/Performance Mon. Basic P, incl. 30 archive tags, for WinCC V7.5, Runtime software, Single license, count relevant, License key download ******************************* E-mail address required for delivery",2702,"ST",1,"SIMATIC",1E-3,1,"6AV63722HG075AA0"]
["6AV6372-2HJ07-4AA0","Sequence execution system, Basic PCKG. incl. 2 units, for SIMATIC WinCC V7.4, Runtime software, Single license, Software and License key download ******************************* E-mail address required for delivery",1654,"ST",1,"SIMATIC",1E-3,1,"6AV63722HJ074AA0"]
["6AV6372-2HJ07-5AA0","Sequence execution system, Basic PCKG. incl. 2 units, for SIMATIC WinCC V7.5, Runtime software, Single license, Software and License key download ******************************* E-mail address required for delivery",1654,"ST",1,"SIMATIC",1E-3,1,"6AV63722HJ075AA0"]
["6AV6372-2HJ17-4AA0","Sequence execution system, Basic PCKG. upgrade, for SIMATIC WinCC V7.4, Runtime software, Single license, Software and License key download ******************************* E-mail address required for delivery",828,"ST",1,"SIMATIC",1E-3,1,"6AV63722HJ174AA0"]
["6AV6372-2HJ17-5AA0","Sequence execution system, Basic PCKG. upgrade, for SIMATIC WinCC V7.5, Runtime software, Single license, Software and License key download ******************************* E-mail address required for delivery",828,"ST",1,"SIMATIC",1E-3,1,"6AV63722HJ175AA0"]
["6AV6372-2HJ17-5AA1","Sequence execution system, Basic PCKG. upgrade, for SIMATIC WinCC V7.5, Runtime software, Single license, Software and License key download",552,"ST",1,"SIMATIC",1E-3,1,"6AV63722HJ175AA1"]
["6AV6372-2JG20-0BA0","WinCC/Performance Mon. ARCH., 30 archive tags, for WinCC V7.2 or higher, Runtime software, Single license, count relevant, License key download ******************************* E-mail address required for delivery",993,"ST",1,"SIMATIC",1E-3,1,"6AV63722JG200BA0"]
["6AV6372-2JG20-0CA0","WinCC/Performance Mon. ARCH., 100 archive tags for WinCC V7.2 or higher, Runtime software, Single license, count relevant, License key download ******************************* E-mail address required for delivery",2977,"ST",1,"SIMATIC",1E-3,1,"6AV63722JG200CA0"]
["6AV6372-2JG20-0DA0","WinCC/Performance Mon. ARCH., 300 archive tags, for WinCC V7.2 or higher, Runtime software, Single license, count relevant, License key download ******************************* E-mail address required for delivery",8038,"ST",1,"SIMATIC",1E-3,1,"6AV63722JG200DA0"]
["6AV6372-2JG20-0EA0","WinCC/Performance Mon. ARCH., 1000 archive tags, for WinCC V7.2 or higher, Runtime software, Single license, count relevant, License key download ******************************* E-mail address required for delivery",26791,"ST",1,"SIMATIC",1E-3,1,"6AV63722JG200EA0"]
["6AV6372-2JJ07-4BA0","Sequence execution system, Extension by 5 units, for SIMATIC WinCC V7.4, Runtime software, Single license, count relevant, License key download ******************************* E-mail address required for delivery",1103,"ST",1,"SIMATIC",1E-3,1,"6AV63722JJ074BA0"]
["6AV6372-2JJ07-5BA0","Sequence execution system, Extension by 5 units, for SIMATIC WinCC V7.5, Runtime software, Single license, count relevant, License key download ******************************* E-mail address required for delivery",1103,"ST",1,"SIMATIC",1E-3,1,"6AV63722JJ075BA0"]
["6AV6372-2JJ17-4BA0","Sequence execution system, extension 5 units upgrade, for SIMATIC WinCC V7.4, Runtime software, Single license, count relevant, License key download ******************************* E-mail address required for delivery",552,"ST",1,"SIMATIC",1E-3,1,"6AV63722JJ174BA0"]
["6AV6372-2JJ17-5BA0","Sequence execution system, extension 5 units upgr from V7.3 to SIMATIC WinCC V7.5, runtime SW, Single license, relevant, License key download ******************************* E-mail address required for delivery",552,"ST",1,"SIMATIC",1E-3,1,"6AV63722JJ175BA0"]
["6AV6372-2JJ17-5BA1","Sequence execution system, extension 5 units upgr from V7.4 to SIMATIC WinCC V7.5, runtime SW, Single license, relevant, License key download ******************************* E-mail address required for delivery",368,"ST",1,"SIMATIC",1E-3,1,"6AV63722JJ175BA1"]
["6AV6372-2KG07-4AX3","WinCC/Performance Mon. Upgrade from V7.X to V7.4, for WinCC V7.4, Runtime software, Single license, License key download ******************************* E-mail address required for delivery",993,"ST",1,"SIMATIC",1E-3,1,"6AV63722KG074AX3"]
["6AV6372-2KG07-5AX3","WinCC/Performance Mon. Upgrade from V7.2/7.3-> V7.5 for WinCC V7.5, Runtime software, Single license, License key download ******************************* E-mail address required for delivery",993,"ST",1,"SIMATIC",1E-3,1,"6AV63722KG075AX3"]
["6AV6372-2KG07-5AX4","WinCC/Performance Mon. Upgrade from V7.4-> V7.5 for WinCC V7.5, Runtime software, Single license, License key download ******************************* E-mail address required for delivery",661,"ST",1,"SIMATIC",1E-3,1,"6AV63722KG075AX4"]
["6AV6372-3DF67-1AA1","SIMATIC Energy Efficiency Package (EM) consisting of: SIMATIC Energy Manager PRO Consumer incl. EE-Monitor V7.1 (6AV6372-2DF67-1AX0), S7 Energy Meter 480 V (6ES7134-6PA20-0BD0), ET 200SP Base Unit (6ES7193-6BP00-0BD0)",520,"ST",1,"SIMATIC",0.31,1,"6AV63723DF671AA1"]
["6AV6372-3DF67-1AA2","SIMATIC Energy Efficiency Package (PAC) consisting of: SIMATIC Energy Manager PRO Consumer incl. EE-Monitor V7.1 (6AV6372-2DF67-1AX0), Sentron PAC 3200 (7KM2112-0BA00-3AA0), Expansion module PROFINET (7KM9300-0AE01-0AA0)",839,"ST",1,"SIMATIC",0.7,1,"6AV63723DF671AA2"]
["6AV6377-1CA07-2AF3","FL migration package WinCC/Server V7.5, option for SIMATIC WinCC V7.5, runtime software, Single License. This is a special offer and is valid if you replace the previously used product FactoryLink with the product WinCC V7.5. By purchasing this product you obligate yourself to replace the previously used product FactoryLink (after a transitional period of 12 months after receiving this product) with WinCC V7.5 and to no longer use the FactoryLink license. For customer with SUS contract",1916,"ST",1,"SIMATIC",0.3,1,"6AV63771CA072AF3"]
["6AV6377-1CB07-2AF3","FL migration package WinCC/User Archive V7.5, option for SIMATIC WinCC V7.5, runtime software, Single License. This is a special offer and is valid if you replace the previously used product FactoryLink with the product WinCC V7.5. By purchasing this product you obligate yourself to replace the previously used product FactoryLink (after a transitional period of 12 months after receiving this product) with WinCC V7.5 and to no longer use the FactoryLink license. For customer with SUS contract",473,"ST",1,"SIMATIC",0.3,1,"6AV63771CB072AF3"]
["6AV6377-1CF07-2AF3","FL migration package WinCC/Redundancy V7.5, option for SIMATIC WinCC V7.5, runtime software, Single License. This is a special offer and is valid if you replace the previously used product FactoryLink with the product WinCC V7.5. By purchasing this product you obligate yourself to replace the previously used product FactoryLink (after a transitional period of 12 months after receiving this product) with WinCC V7.5 and to no longer use the FactoryLink license. For customer with SUS contract",1986,"ST",1,"SIMATIC",0.3,1,"6AV63771CF072AF3"]
["6AV6377-1DH07-4AF3","FL migration package WinCC/Web Navigator V7.5, 3 client licenses (countable), option for WinCC V7.5 or higher This is a special offer and is valid if you replace the previously used product FactoryLink with the product WinCC V7.5. By purchasing this product you obligate yourself to replace the previously used product FactoryLink (following a transitional period of 12 months after receiving this product) with WinCC V7.5 and to no longer use the FactoryLink license. For customers with SUS contract ******************************* Content: 6AV6362-1AD00-0BB0",3902,"ST",1,"SIMATIC",0.3,1,"6AV63771DH074AF3"]
["6AV6377-1DH07-4BF3","FL migration package WinCC/Web Navigator V7.5, 10 client licenses (countable), option for WinCC V7.5 or higher This is a special offer and is valid if you replace the previously used product FactoryLink with the product WinCC V7.5. By purchasing this product you obligate yourself to replace the previously used product FactoryLink (following a transitional period of 12 months after receiving this product) with WinCC V7.5 and to no longer use the FactoryLink license. For customers with SUS contract ******************************* Content: 6AV6362-1AF00-0BB0",6810,"ST",1,"SIMATIC",0.3,1,"6AV63771DH074BF3"]
["6AV6377-1DH07-4CF3","FL migration package WinCC/Web Navigator V7.5, 30 client licenses (countable), option for WinCC V7.5 or higher This is a special offer and is valid if you replace the previously used product FactoryLink with the product WinCC V7.5. By purchasing this product you obligate yourself to replace the previously used product FactoryLink (following a transitional period of 12 months after receiving this product) with WinCC V7.5 and to no longer use the FactoryLink license. For customers with SUS contract ******************************* Content: 6AV6362-1AJ00-0BB0",16720,"ST",1,"SIMATIC",0.3,1,"6AV63771DH074CF3"]
["6AV6381-1AA00-0AX5","WinCC Software Update Service, valid for 1 license Automatic subsequent deliveries of Upgrades and service packs within the framework of this contract, you will receive for one year all up-to-date software versions. the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software",1120,"ST",1,"SIMATIC",1.4999999999999999E-2,1,"6AV63811AA000AX5"]
["6AV6381-1AA00-0BX5","WinCC Software Update Service, valid for 3 licenses Automatic subsequent deliveries of Upgrades and service packs within the framework of this contract, you will receive for one year all up-to-date software versions. the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software",2720,"ST",1,"SIMATIC",1.4999999999999999E-2,1,"6AV63811AA000BX5"]
["6AV6381-1AA00-0CX5","WinCC Software Update Service, valid for 10 licenses Automatic subsequent deliveries of Upgrades and service packs within the framework of this contract, you will receive for one year all up-to-date software versions. the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software",7462,"ST",1,"SIMATIC",1.4999999999999999E-2,1,"6AV63811AA000CX5"]
["6AV6381-1BP07-4AX3","Upgrade Trainer Package WinCC including Web Navigator V7.4, includes: SW and documentation on DVD, 6-unit license on USB stick Upgrade to WinCC V7.4 RC 2048 and Web Navigator, for educational purposes only",975,"ST",1,"SIMATIC",0.251,1,"6AV63811BP074AX3"]
["6AV6381-1BP07-5AX3","Upgrade Trainer Package WinCC including Web Navigator V7.5, includes: SW and documentation on DVD, 6-unit license on USB stick Upgrade to WinCC V7.5 RC 2048 and Web Navigator, Diagnostics Client for educational purposes only",975,"ST",1,"SIMATIC",0.30099999999999999,1,"6AV63811BP075AX3"]
["6AV6381-1KA00-0AX5","WinCC Software Update Service Download valid for 1 license, Automatic subsequent deliveries of Upgrades and service packs within the framework of this contract, you will receive for one year all up-to-date software versions. the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software ****************************** E-mail address required for delivery",996,"ST",1,"SIMATIC",1E-3,1,"6AV63811KA000AX5"]
["6AV6381-1KA00-0BX5","WinCC Software Update Service Download valid for 3 licenses Automatic subsequent deliveries of Upgrades and service packs within the framework of this contract, you will receive for one year all up-to-date software versions. the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software ****************************** E-mail address required for delivery",2419,"ST",1,"SIMATIC",1E-3,1,"6AV63811KA000BX5"]
["6AV6381-1KA00-0CX5","WinCC Software Update Service Download valid for 10 licenses Automatic subsequent deliveries of Upgrades and service packs within the framework of this contract, you will receive for one year all up-to-date software versions. the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software ****************************** E-mail address required for delivery",6635,"ST",1,"SIMATIC",1E-3,1,"6AV63811KA000CX5"]
["6AV6381-1XX07-0AP0","EPL master for WinCC V7 (EPL=Enterprise License) Mandatory royalty per 1 installation only valid in connection with Enterprise License contract",1789,"ST",1,"SIMATIC",0.94499999999999995,1,"6AV63811XX070AP0"]
["6AV6381-1XX07-4AP0","EPL master for WinCC V7.4 SP1, (EPL=Enterprise License) Mandatory royalty per 1 installation only valid in connection with Enterprise License contract",1688,"ST",1,"SIMATIC",0.32400000000000001,1,"6AV63811XX074AP0"]
["6AV6381-1XX07-5AP0","EPL master for WinCC V7.5, (EPL=Enterprise License) Royalty obligation for each installation! Only valid in connection with Enterprise License contract",1688,"ST",1,"SIMATIC",0.42399999999999999,1,"6AV63811XX075AP0"]
["6AV6381-2AA07-4AK3","SIMATIC WinCC RT Upgrade from V7.X to V7.4 SP1 for SIMATIC WinCC Runtime (RT) incl. options redundancy, server, User archive, Web Navigator, Web NAV Load-Balancing, Web diagnostics client/server, Data Monitor, Connectivity Pack, Connectivity Station, Runtime/Configuration software, Single license, SW and License Key Download ******************************* E-mail address required for delivery",956,"ST",1,"SIMATIC",1E-3,1,"6AV63812AA074AK3"]
["6AV6381-2AA07-4AV3","SIMATIC WinCC RT Upgrade Asia from V7.X to V7.4 SP1 for SIMATIC WinCC Runtime (RT) incl. options Redundancy, Server, User Archive, Web Navigator, Web NAV Load-Balancing, Web Diagnostics Client/Server, Data Monitor, Connectivity Pack, Connectivity Station Runtime/configuration software on DVD, single license, license key on USB flash drive ******************************* Content: Set (2x DVD + 1x USB)",1076,"ST",1,"SIMATIC",0.26700000000000002,1,"6AV63812AA074AV3"]
["6AV6381-2AA07-4AX3","SIMATIC WinCC RT Upgrade from V7.X to V7.4 SP1 for SIMATIC WinCC Runtime (RT) incl. options Redundancy, Server, User Archive, Web Navigator, Web NAV Load-Balancing, Web Diagnostics Client/Server, Data Monitor, Connectivity Pack, Connectivity Station, Runtime/configuration software on DVD, single license, license key on USB flash drive ******************************* Content: Set (2x DVD + 1x USB)",1076,"ST",1,"SIMATIC",0.26300000000000001,1,"6AV63812AA074AX3"]
["6AV6381-2AA07-5AK3","SIMATIC WinCC RT SW upgrade from V7.2/7.3 to V7.5 for SIMATIC WinCC Runtime (RT) incl. options Redundancy, server, user archive, Web Navigator, Web NAV Load-Balancing, web diagnostics client/server, Data Monitor, Connectivity Pack, Connectivity Station, runtime/configuration software, Single license, SW and license key download ******************************* E-mail address required for delivery",956,"ST",1,"SIMATIC",1E-3,1,"6AV63812AA075AK3"]
["6AV6381-2AA07-5AK4","SIMATIC WinCC RT SW upgrade from V7.4 to V7.5 for SIMATIC WinCC Runtime (RT) incl. options Redundancy, server, user archive, Web Navigator, Web NAV Load-Balancing, web diagnostics client/server, Data Monitor, Connectivity Pack, Connectivity Station, runtime/configuration software, Single license, SW and license key download ******************************* E-mail address required for delivery",676,"ST",1,"SIMATIC",1E-3,1,"6AV63812AA075AK4"]
["6AV6381-2AA07-5AV3","SIMATIC WinCC RT SW Upgrade Asia from V7.2/7.3 to V7.5 for SIMATIC WinCC Runtime (RT) incl. options Redundancy, Server, User Archive, Web Navigator, Web NAV Load-Balancing, Web Diagnostics Client/Server, Data Monitor, Connectivity Pack, Connectivity Station Runtime/configuration software on DVD, single license, license key on USB flash drive ******************************* Content: Set (3x DVD + 1x USB)",1076,"ST",1,"SIMATIC",0.317,1,"6AV63812AA075AV3"]
["6AV6381-2AA07-5AV4","SIMATIC WinCC RT SW Upgrade Asia from V7.4 to V7.5 for SIMATIC WinCC Runtime (RT) incl. options Redundancy, Server, User Archive, Web Navigator, Web NAV Load-Balancing, Web Diagnostics Client/Server, Data Monitor, Connectivity Pack, Connectivity Station Runtime/configuration software on DVD, single license, license key on USB flash drive ******************************* Content: Set (3x DVD + 1x USB)",760,"ST",1,"SIMATIC",0.317,1,"6AV63812AA075AV4"]
["6AV6381-2AA07-5AX3","SIMATIC WinCC RT SW Upgrade from V7.2/7.3 to V7.5 for SIMATIC WinCC Runtime (RT) incl. options Redundancy, Server, User Archive, Web Navigator, Web NAV Load-Balancing, Web Diagnostics Client/Server, Data Monitor, Connectivity Pack, Connectivity Station Runtime/configuration software on DVD, single license, license key on USB flash drive ******************************* Content: Set (3x DVD + 1x USB)",1076,"ST",1,"SIMATIC",0.313,1,"6AV63812AA075AX3"]
["6AV6381-2AA07-5AX4","SIMATIC WinCC RT SW Upgrade from V7.4 to V7.5 for SIMATIC WinCC Runtime (RT) incl. options Redundancy, Server, User Archive, Web Navigator, Web NAV Load-Balancing, Web Diagnostics Client/Server, Data Monitor, Connectivity Pack, Connectivity Station Runtime/configuration software on DVD, single license, license key on USB flash drive ******************************* Content: Set (3x DVD + 1x USB)",760,"ST",1,"SIMATIC",0.313,1,"6AV63812AA075AX4"]
["6AV6381-2AB07-4AK3","SIMATIC WinCC RC Upgrade, from V7.X to V7.4 SP1 for SIMATIC WinCC Runtime & Configuration (RC) incl. options redundancy, server, User archive, Web Navigator, Web NAV Load-Balancing, Web diagnostics client/server, Data Monitor, Connectivity Pack, Connectivity Station, Runtime/Configuration software, Single license, SW and License Key Download ******************************* E-mail address required for delivery",1676,"ST",1,"SIMATIC",1E-3,1,"6AV63812AB074AK3"]
["6AV6381-2AB07-4AV3","SIMATIC WinCC RC Upgrade Asia from V7.X to V7.4 SP1 for SIMATIC WinCC Runtime & Configuration (RC), incl. options Redundancy, Server, User Archive, Web Navigator, Web NAV Load-Balancing, Web Diagnostics Client/Server, Data Monitor, Connectivity Pack, Connectivity Station Runtime/configuration software on DVD, single license, license key on USB flash drive ******************************* Content: Set (2x DVD + 1x USB)",1885,"ST",1,"SIMATIC",0.26700000000000002,1,"6AV63812AB074AV3"]
["6AV6381-2AB07-4AX3","SIMATIC WinCC RC Upgrade, from V7.X to V7.4 SP1 for SIMATIC WinCC Runtime & Configuration (RC) incl. options Redundancy, Server, User Archive, Web Navigator, Web NAV Load-Balancing, Web Diagnostics Client/Server, Data Monitor, Connectivity Pack, Connectivity Station, Runtime/configuration software on DVD, single license, license key on USB flash drive ******************************* Content: Set (2x DVD + 1x USB)",1885,"ST",1,"SIMATIC",0.26300000000000001,1,"6AV63812AB074AX3"]
["6AV6381-2AB07-5AK3","SIMATIC WinCC RC SW upgrade from V7.2/7.3 to V7.5 for SIMATIC WinCC Runtime & Configuration (RC) incl. options Redundancy, server, user archive, Web Navigator, Web NAV Load-Balancing, web diagnostics client/server, Data Monitor, Connectivity Pack, Connectivity Station, runtime/configuration software, Single license, SW and license key download ******************************* E-mail address required for delivery",1676,"ST",1,"SIMATIC",1E-3,1,"6AV63812AB075AK3"]
["6AV6381-2AB07-5AK4","SIMATIC WinCC RC SW upgrade from V7.4 to V7.5 for SIMATIC WinCC Runtime & Configuration (RC) incl. options Redundancy, server, user archive, Web Navigator, Web NAV Load-Balancing, web diagnostics client/server, Data Monitor, Connectivity Pack, Connectivity Station, runtime/configuration software, Single license, SW and license key download ******************************* E-mail address required for delivery",1113,"ST",1,"SIMATIC",1E-3,1,"6AV63812AB075AK4"]
["6AV6381-2AB07-5AV3","SIMATIC WinCC RC SW Upgrade Asia from V7.2/7.3 to V7.5 for SIMATIC WinCC Runtime & Configuration (RC), incl. options Redundancy, Server, User Archive, Web Navigator, Web NAV Load-Balancing, Web Diagnostics Client/Server, Data Monitor, Connectivity Pack, Connectivity Station Runtime/configuration software on DVD, single license, license key on USB flash drive ******************************* Content: Set (3x DVD + 1x USB)",1885,"ST",1,"SIMATIC",0.317,1,"6AV63812AB075AV3"]
["6AV6381-2AB07-5AV4","SIMATIC WinCC RC SW Upgrade Asia from V7.4 to V7.5 for SIMATIC WinCC Runtime & Configuration (RC), incl. options Redundancy, Server, User Archive, Web Navigator, Web NAV Load-Balancing, Web Diagnostics Client/Server, Data Monitor, Connectivity Pack, Connectivity Station Runtime/configuration software on DVD, single license, license key on USB flash drive ******************************* Content: Set (3x DVD + 1x USB)",1252,"ST",1,"SIMATIC",0.317,1,"6AV63812AB075AV4"]
["6AV6381-2AB07-5AX3","SIMATIC WinCC RC SW Upgrade from V7.2/7.3 to V7.5 for SIMATIC WinCC Runtime & Configuration (RC), incl. options Redundancy, Server, User Archive, Web Navigator, Web NAV Load-Balancing, Web Diagnostics Client/Server, Data Monitor, Connectivity Pack, Connectivity Station Runtime/configuration software on DVD, single license, license key on USB flash drive ******************************* Content: Set (3x DVD + 1x USB)",1885,"ST",1,"SIMATIC",0.313,1,"6AV63812AB075AX3"]
["6AV6381-2AB07-5AX4","SIMATIC WinCC RC SW Upgrade from V7.4 to V7.5 for SIMATIC WinCC Runtime & Configuration (RC), incl. options Redundancy, Server, User Archive, Web Navigator, Web NAV Load-Balancing, Web Diagnostics Client/Server, Data Monitor, Connectivity Pack, Connectivity Station Runtime/configuration software on DVD, single license, license key on USB flash drive ******************************* Content: Set (3x DVD + 1x USB)",1252,"ST",1,"SIMATIC",0.313,1,"6AV63812AB075AX4"]
["6AV6381-2BC07-0AQ0","EPL Royalty for WinCC V7, RT 128 (128 PowerTags) only valid in connection with Enterprise License agreement, requires EPL Master",2379,"ST",1,"SIMATIC",1.2E-2,1,"6AV63812BC070AQ0"]
["6AV6381-2BC07-4AH0","WinCC system software V7.4 SP1, RT 128 (128 Power Tags), runtime software, single license, SW and license key download Class A, 5 languages (de,en,fr,es,it), executable in Windows 7 Prof/Ent/Ult +SP1 (32 bit)/ 7 Prof/Ent/Ult +SP1 (64 bit)/ 8.1 Prof./Ent (32 bit)/ 8.1 Prof./Ent (64 bit)/ 10 Prof./Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 (64 bit)/ Server 2016 (64 bit) ******************************* E-mail address required for delivery",2379,"ST",1,"SIMATIC",1E-3,1,"6AV63812BC074AH0"]
["6AV6381-2BC07-4AV0","WinCC System SW V7.4 SP1 Asia, RT 128 (128 PowerTags), runtime software, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 9 languages (de,en,fr,es,it, zh-s,zh-t,kor,jpn), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",2675,"ST",1,"SIMATIC",0.26700000000000002,1,"6AV63812BC074AV0"]
["6AV6381-2BC07-4AX0","WinCC system software V7.4 SP1, RT 128 (128 PowerTags), runtime software, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",2675,"ST",1,"SIMATIC",0.26300000000000001,1,"6AV63812BC074AX0"]
["6AV6381-2BC07-5AH0","WinCC system software V7.5, RT 128 (128 PowerTags) runtime software, single license, SW incl. documentation and license key download, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* E-mail address required for delivery",2379,"ST",1,"SIMATIC",1E-3,1,"6AV63812BC075AH0"]
["6AV6381-2BC07-5AV0","WinCC System SW V7.5 Asia, RT 128 (128 PowerTags) runtime software, single license, SW and documentation on DVD, License key on USB stick, Class A, 9 languages (de, en,fr,es,it,zh-s,zh-t,kor,jpn), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",2675,"ST",1,"SIMATIC",0.317,1,"6AV63812BC075AV0"]
["6AV6381-2BC07-5AX0","WinCC system software V7.5, RT 128 (128 PowerTags) runtime software, single license, SW and documentation on DVD, License key on USB stick, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",2675,"ST",1,"SIMATIC",0.313,1,"6AV63812BC075AX0"]
["6AV6381-2BD07-4AH0","WinCC system software V7.4 SP1, RT 512 (512 Power Tags), runtime software, single license, SW and license key download Class A, 5 languages (de,en,fr,es,it), executable in Windows 7 Prof/Ent/Ult +SP1 (32 bit)/ 7 Prof/Ent/Ult +SP1 (64 bit)/ 8.1 Prof./Ent (32 bit)/ 8.1 Prof./Ent (64 bit)/ 10 Prof./Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 (64 bit)/ Server 2016 (64 bit) ******************************* E-mail address required for delivery",3656,"ST",1,"SIMATIC",1E-3,1,"6AV63812BD074AH0"]
["6AV6381-2BD07-4AV0","WinCC System SW V7.4 SP1 Asia, RT 512 (512 PowerTags), runtime software, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 9 languages (de,en,fr,es,it, zh-s,zh-t,kor,jpn), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",4111,"ST",1,"SIMATIC",0.26700000000000002,1,"6AV63812BD074AV0"]
["6AV6381-2BD07-4AX0","WinCC system software V7.4 SP1, RT 512 (512 PowerTags), runtime software, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",4111,"ST",1,"SIMATIC",0.26300000000000001,1,"6AV63812BD074AX0"]
["6AV6381-2BD07-5AH0","WinCC system software V7.5, RT 512 (512 PowerTags), runtime software, single license, SW incl. documentation and license key download, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* E-mail address required for delivery",3656,"ST",1,"SIMATIC",1E-3,1,"6AV63812BD075AH0"]
["6AV6381-2BD07-5AV0","WinCC System SW V7.5 Asia, RT 512 (512 PowerTags), runtime software, single license, SW and documentation on DVD, License key on USB stick, Class A, 9 languages (de, en,fr,es,it,zh-s,zh-t,kor,jpn), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",4111,"ST",1,"SIMATIC",0.317,1,"6AV63812BD075AV0"]
["6AV6381-2BD07-5AX0","WinCC system software V7.5, RT 512 (512 PowerTags), runtime software, single license, SW and documentation on DVD, License key on USB stick, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",4111,"ST",1,"SIMATIC",0.313,1,"6AV63812BD075AX0"]
["6AV6381-2BE07-4AH0","WinCC system software V7.4 SP1, RT 2048 (2048 Power Tags), runtime software, single license, SW and license key download Class A, 5 languages (de,en,fr,es,it), executable in Windows 7 Prof/Ent/Ult +SP1 (32 bit)/ 7 Prof/Ent/Ult +SP1 (64 bit)/ 8.1 Prof./Ent (32 bit)/ 8.1 Prof./Ent (64 bit)/ 10 Prof./Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 (64 bit)/ Server 2016 (64 bit) ******************************* E-mail address required for delivery",4494,"ST",1,"SIMATIC",1E-3,1,"6AV63812BE074AH0"]
["6AV6381-2BE07-4AV0","WinCC System SW V7.4 SP1 Asia, RT 2048 (2048 PowerTags), runtime software, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 9 languages (de,en,fr,es,it, zh-s,zh-t,kor,jpn), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",5054,"ST",1,"SIMATIC",0.26700000000000002,1,"6AV63812BE074AV0"]
["6AV6381-2BE07-4AX0","WinCC system software V7.4 SP1, RT 2048 (2048 PowerTags), runtime software, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",5054,"ST",1,"SIMATIC",0.26300000000000001,1,"6AV63812BE074AX0"]
["6AV6381-2BE07-5AH0","WinCC system software V7.5, RT 2048 (2048 PowerTags), runtime software, single license, SW incl. documentation and license key download, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* E-mail address required for delivery",4494,"ST",1,"SIMATIC",1E-3,1,"6AV63812BE075AH0"]
["6AV6381-2BE07-5AV0","WinCC System SW V7.5 Asia, RT 2048 (2048 PowerTags), runtime software, single license, SW and documentation on DVD, License key on USB stick, Class A, 9 languages (de, en,fr,es,it,zh-s,zh-t,kor,jpn), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",5054,"ST",1,"SIMATIC",0.317,1,"6AV63812BE075AV0"]
["6AV6381-2BE07-5AX0","WinCC system software V7.5, RT 2048 (2048 PowerTags), runtime software, single license, SW and documentation on DVD, License key on USB stick, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",5054,"ST",1,"SIMATIC",0.313,1,"6AV63812BE075AX0"]
["6AV6381-2BF07-0AQ0","EPL Royalty for WinCC V7, RT65535 (65535 PowerTags) only valid in connection with Enterprise License agreement, requires EPL Master",6635,"ST",1,"SIMATIC",1.2E-2,1,"6AV63812BF070AQ0"]
["6AV6381-2BF07-4AH0","WinCC system software V7.4 SP1, RT 65536 (65536 Power Tags), runtime software, single license, SW and license key download Class A, 5 languages (de,en,fr,es,it), executable in Windows 7 Prof/Ent/Ult +SP1 (32 bit)/ 7 Prof/Ent/Ult +SP1 (64 bit)/ 8.1 Prof./Ent (32 bit)/ 8.1 Prof./Ent (64 bit)/ 10 Prof./Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 (64 bit)/ Server 2016 (64 bit) ******************************* E-mail address required for delivery",6635,"ST",1,"SIMATIC",1E-3,1,"6AV63812BF074AH0"]
["6AV6381-2BF07-4AV0","WinCC System SW V7.4 SP1 Asia, RT 65536 (65536 PowerTags), runtime software, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 9 languages (de,en,fr,es,it, zh-s,zh-t,kor,jpn), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",7462,"ST",1,"SIMATIC",0.26700000000000002,1,"6AV63812BF074AV0"]
["6AV6381-2BF07-4AX0","WinCC system software V7.4 SP1, RT 65536 (65536 PowerTags), runtime software, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",7462,"ST",1,"SIMATIC",0.26300000000000001,1,"6AV63812BF074AX0"]
["6AV6381-2BF07-5AH0","WinCC system software V7.5, RT 65536 (65536 PowerTags), runtime software, single license, SW incl. documentation and license key download, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* E-mail address required for delivery",6635,"ST",1,"SIMATIC",1E-3,1,"6AV63812BF075AH0"]
["6AV6381-2BF07-5AV0","WinCC System SW V7.5 Asia, RT 65536 (65536 PowerTags), runtime software, single license, SW and documentation on DVD, License key on USB stick, Class A, 9 languages (de, en,fr,es,it,zh-s,zh-t,kor,jpn), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",7462,"ST",1,"SIMATIC",0.317,1,"6AV63812BF075AV0"]
["6AV6381-2BF07-5AX0","WinCC system software V7.5, RT 65536 (65536 PowerTags), runtime software, single license, SW and documentation on DVD, License key on USB stick, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",7462,"ST",1,"SIMATIC",0.313,1,"6AV63812BF075AX0"]
["6AV6381-2BH07-0AQ0","EPL Royalty for WinCC V7, RT8192 (8192 PowerTags) only valid in connection with Enterprise License agreement, requires EPL Master",5397,"ST",1,"SIMATIC",1.2E-2,1,"6AV63812BH070AQ0"]
["6AV6381-2BH07-4AH0","WinCC system software V7.4 SP1, RT 8192 (8192 Power Tags), runtime software, single license, SW and license key download Class A, 5 languages (de,en,fr,es,it), executable in Windows 7 Prof/Ent/Ult +SP1 (32 bit)/ 7 Prof/Ent/Ult +SP1 (64 bit)/ 8.1 Prof./Ent (32 bit)/ 8.1 Prof./Ent (64 bit)/ 10 Prof./Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 (64 bit)/ Server 2016 (64 bit) ******************************* E-mail address required for delivery",5397,"ST",1,"SIMATIC",1E-3,1,"6AV63812BH074AH0"]
["6AV6381-2BH07-4AV0","WinCC System SW V7.4 SP1 Asia, RT 8192 (8192 PowerTags), runtime software, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 9 languages (de,en,fr,es,it, zh-s,zh-t,kor,jpn), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",6069,"ST",1,"SIMATIC",0.26700000000000002,1,"6AV63812BH074AV0"]
["6AV6381-2BH07-4AX0","WinCC system software V7.4 SP1, RT 8192 (8192 PowerTags), runtime software, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",6069,"ST",1,"SIMATIC",0.26300000000000001,1,"6AV63812BH074AX0"]
["6AV6381-2BH07-5AH0","WinCC system software V7.5, RT 8192 (8192 PowerTags), runtime software, single license, SW incl. documentation and license key download, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* E-mail address required for delivery",5397,"ST",1,"SIMATIC",1E-3,1,"6AV63812BH075AH0"]
["6AV6381-2BH07-5AV0","WinCC System SW V7.5 Asia, RT 8192 (8192 PowerTags), runtime software, single license, SW and documentation on DVD, License key on USB stick, Class A, 9 languages (de, en,fr,es,it,zh-s,zh-t,kor,jpn), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",6069,"ST",1,"SIMATIC",0.317,1,"6AV63812BH075AV0"]
["6AV6381-2BH07-5AX0","WinCC system software V7.5, RT 8192 (8192 PowerTags), runtime software, single license, SW and documentation on DVD, License key on USB stick, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",6069,"ST",1,"SIMATIC",0.313,1,"6AV63812BH075AX0"]
["6AV6381-2BJ07-4AH0","WinCC system software V7.4 SP1, RT 102400 (102400 Power Tags), runtime software, single license, SW and license key download Class A, 5 languages (de,en,fr,es,it), executable in Windows 7 Prof/Ent/Ult +SP1 (32 bit)/ 7 Prof/Ent/Ult +SP1 (64 bit)/ 8.1 Prof./Ent (32 bit)/ 8.1 Prof./Ent (64 bit)/ 10 Prof./Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 (64 bit)/ Server 2016 (64 bit) ******************************* E-mail address required for delivery",9334,"ST",1,"SIMATIC",1E-3,1,"6AV63812BJ074AH0"]
["6AV6381-2BJ07-4AV0","WinCC System SW V7.4 SP1 Asia, RT 102400 (102400 PowerTags), runtime software, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 9 languages (de,en,fr,es,it, zh-s,zh-t,kor,jpn), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",10496,"ST",1,"SIMATIC",0.26700000000000002,1,"6AV63812BJ074AV0"]
["6AV6381-2BJ07-4AX0","WinCC system software V7.4 SP1, RT 102400 (102400 PowerTags), runtime software, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",10496,"ST",1,"SIMATIC",0.26300000000000001,1,"6AV63812BJ074AX0"]
["6AV6381-2BJ07-5AH0","WinCC system software V7.5, RT 102400 (102400 PowerTags), runtime software, single license, SW incl. documentation and license key download, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* E-mail address required for delivery",9334,"ST",1,"SIMATIC",1E-3,1,"6AV63812BJ075AH0"]
["6AV6381-2BJ07-5AV0","WinCC System SW V7.5 Asia, RT 102400 (102400 PowerTags), runtime software, single license, SW and documentation on DVD, License key on USB stick, Class A, 9 languages (de, en,fr,es,it,zh-s,zh-t,kor,jpn), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",10496,"ST",1,"SIMATIC",0.317,1,"6AV63812BJ075AV0"]
["6AV6381-2BJ07-5AX0","WinCC system software V7.5, RT 102400 (102400 PowerTags), runtime software, single license, SW and documentation on DVD, License key on USB stick, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",10496,"ST",1,"SIMATIC",0.313,1,"6AV63812BJ075AX0"]
["6AV6381-2BK07-4AH0","WinCC system software V7.4 SP1, RT 153600 (153600 Power Tags), runtime software, single license, SW and license key download Class A, 5 languages (de,en,fr,es,it), executable in Windows 7 Prof/Ent/Ult +SP1 (32 bit)/ 7 Prof/Ent/Ult +SP1 (64 bit)/ 8.1 Prof./Ent (32 bit)/ 8.1 Prof./Ent (64 bit)/ 10 Prof./Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 (64 bit)/ Server 2016 (64 bit) ******************************* E-mail address required for delivery",12146,"ST",1,"SIMATIC",1E-3,1,"6AV63812BK074AH0"]
["6AV6381-2BK07-4AV0","WinCC System SW V7.4 SP1 Asia, RT 153600 (153600 PowerTags), runtime software, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 9 languages (de,en,fr,es,it, zh-s,zh-t,kor,jpn), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",13658,"ST",1,"SIMATIC",0.26700000000000002,1,"6AV63812BK074AV0"]
["6AV6381-2BK07-4AX0","WinCC system software V7.4 SP1, RT 153600 (153600 PowerTags), runtime software, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",13658,"ST",1,"SIMATIC",0.26300000000000001,1,"6AV63812BK074AX0"]
["6AV6381-2BK07-5AH0","WinCC system software V7.5, RT 153600 (153600 PowerTags), runtime software, single license, SW incl. documentation and license key download, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* E-mail address required for delivery",12146,"ST",1,"SIMATIC",1E-3,1,"6AV63812BK075AH0"]
["6AV6381-2BK07-5AV0","WinCC System SW V7.5 Asia, RT 153600 (153600 PowerTags), runtime software, single license, SW and documentation on DVD, License key on USB stick, Class A, 9 languages (de, en,fr,es,it,zh-s,zh-t,kor,jpn), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",13659,"ST",1,"SIMATIC",0.317,1,"6AV63812BK075AV0"]
["6AV6381-2BK07-5AX0","WinCC system software V7.5, RT 153600 (153600 PowerTags), runtime software, single license, SW and documentation on DVD, License key on USB stick, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",13659,"ST",1,"SIMATIC",0.313,1,"6AV63812BK075AX0"]
["6AV6381-2BL07-4AH0","WinCC system software V7.4 SP1, RT 262144 (262144 Power Tags), runtime software, single license, SW and license key download Class A, 5 languages (de,en,fr,es,it), executable in Windows 7 Prof/Ent/Ult +SP1 (32 bit)/ 7 Prof/Ent/Ult +SP1 (64 bit)/ 8.1 Prof./Ent (32 bit)/ 8.1 Prof./Ent (64 bit)/ 10 Prof./Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 (64 bit)/ Server 2016 (64 bit) ******************************* E-mail address required for delivery",16643,"ST",1,"SIMATIC",1E-3,1,"6AV63812BL074AH0"]
["6AV6381-2BL07-4AV0","WinCC System SW V7.4 SP1 Asia, RT 262144 (262144 PowerTags), runtime software, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 9 languages (de,en,fr,es,it, zh-s,zh-t,kor,jpn), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",18717,"ST",1,"SIMATIC",0.26700000000000002,1,"6AV63812BL074AV0"]
["6AV6381-2BL07-4AX0","WinCC system software V7.4 SP1, RT 262144 (262144 PowerTags), runtime software, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Std/Prof/Ent/Ult (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",18717,"ST",1,"SIMATIC",0.26300000000000001,1,"6AV63812BL074AX0"]
["6AV6381-2BL07-5AH0","WinCC system software V7.5, RT 262144 (262144 PowerTags), runtime software, single license, SW incl. documentation and license key download, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* E-mail address required for delivery",16643,"ST",1,"SIMATIC",1E-3,1,"6AV63812BL075AH0"]
["6AV6381-2BL07-5AV0","WinCC System SW V7.5 Asia, RT 262144 (262144 PowerTags), runtime software, single license, SW and documentation on DVD, License key on USB stick, Class A, 9 languages (de, en,fr,es,it,zh-s,zh-t,kor,jpn), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",18718,"ST",1,"SIMATIC",0.317,1,"6AV63812BL075AV0"]
["6AV6381-2BL07-5AX0","WinCC system software V7.5, RT 262144 (262144 PowerTags), runtime software, single license, SW and documentation on DVD, License key on USB stick, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 8.1 STD/Prof/Ent/Ult (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 (64 bit) ******************************* Content: set (3x DVD + 1x USB)",18718,"ST",1,"SIMATIC",0.313,1,"6AV63812BL075AX0"]
["6AV6381-2BM07-0AQ0","EPL Royalty for WinCC V7, RC128 (128 PowerTags) only valid in connection with Enterprise License agreement, requires EPL Master",3565,"ST",1,"SIMATIC",1.2E-2,1,"6AV63812BM070AQ0"]
["6AV6381-2BM07-4AH0","WinCC system software V7.4 SP1, RC 128 (128 Power Tags), Runtime/Configuration software, floating license, SW and license key download Class A, 5 languages (de,en,fr,es,it), executable in Windows 7 Prof/Ent/Ult +SP1 (32 bit)/ 7 Prof/Ent/Ult +SP1 (64 bit)/ 8.1 Prof./Ent (32 bit)/ 8.1 Prof./Ent (64 bit)/ 10 Prof./Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 (64 bit)/ Server 2016 (64 bit) ******************************* E-mail address required for delivery",3565,"ST",1,"SIMATIC",1E-3,1,"6AV63812BM074AH0"]
["6AV6381-2BM07-4AV0","WinCC System SW V7.4 SP1 Asia, RC 128 (128 PowerTags), Runtime/configuration software on DVD, floating license, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",4009,"ST",1,"SIMATIC",0.26700000000000002,1,"6AV63812BM074AV0"]
["6AV6381-2BM07-4AX0","WinCC system software V7.4 SP1, RC 128 (128 PowerTags), Runtime/configuration software on DVD, floating license, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",4009,"ST",1,"SIMATIC",0.26300000000000001,1,"6AV63812BM074AX0"]
["6AV6381-2BM07-5AH0","WinCC system software V7.5, RC 128 (128 PowerTags) Runtime/Configuration software, floating license, SW incl. docu. and license key download, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* E-mail address required for delivery",3565,"ST",1,"SIMATIC",1E-3,1,"6AV63812BM075AH0"]
["6AV6381-2BM07-5AV0","WinCC System SW V7.5 Asia, RC 128 (128 PowerTags) Runtime/Configuration software on DVD, floating license, License key on USB stick, Class A, 9 languages (de, en,fr,es,it,zh-s,zh-t,kor,jpn), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",4010,"ST",1,"SIMATIC",0.317,1,"6AV63812BM075AV0"]
["6AV6381-2BM07-5AX0","WinCC system software V7.5, RC 128 (128 PowerTags) Runtime/Configuration software on DVD, floating license, License key on USB stick, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",4010,"ST",1,"SIMATIC",0.313,1,"6AV63812BM075AX0"]
["6AV6381-2BN07-0AQ0","EPL Royalty for WinCC V7, RC512 (512 PowerTags) only valid in connection with Enterprise License agreement, requires EPL Master",6073,"ST",1,"SIMATIC",1.2E-2,1,"6AV63812BN070AQ0"]
["6AV6381-2BN07-4AH0","WinCC system software V7.4 SP1, RC 512 (512 Power Tags), Runtime/Configuration software, floating license, SW and license key download Class A, 5 languages (de,en,fr,es,it), executable in Windows 7 Prof/Ent/Ult +SP1 (32 bit)/ 7 Prof/Ent/Ult +SP1 (64 bit)/ 8.1 Prof./Ent (32 bit)/ 8.1 Prof./Ent (64 bit)/ 10 Prof./Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 (64 bit)/ Server 2016 (64 bit) ******************************* E-mail address required for delivery",6073,"ST",1,"SIMATIC",1E-3,1,"6AV63812BN074AH0"]
["6AV6381-2BN07-4AV0","WinCC System SW V7.4 SP1 Asia, RC 512 (512 PowerTags), Runtime/configuration software on DVD, floating license, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",6830,"ST",1,"SIMATIC",0.26700000000000002,1,"6AV63812BN074AV0"]
["6AV6381-2BN07-4AX0","WinCC system software V7.4 SP1, RC 512 (512 PowerTags), Runtime/configuration software on DVD, floating license, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",6830,"ST",1,"SIMATIC",0.26300000000000001,1,"6AV63812BN074AX0"]
["6AV6381-2BN07-5AH0","WinCC system software V7.5, RC 512 (512 PowerTags), Runtime/Configuration software, floating license, SW incl. docu. and license key download, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* E-mail address required for delivery",6073,"ST",1,"SIMATIC",1E-3,1,"6AV63812BN075AH0"]
["6AV6381-2BN07-5AV0","WinCC System SW V7.5 Asia, RC 512 (512 PowerTags), Runtime/Configuration software on DVD, floating license, License key on USB stick, Class A, 9 languages (de, en,fr,es,it,zh-s,zh-t,kor,jpn), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",6830,"ST",1,"SIMATIC",0.317,1,"6AV63812BN075AV0"]
["6AV6381-2BN07-5AX0","WinCC system software V7.5, RC 512 (512 PowerTags), Runtime/Configuration software on DVD, floating license, License key on USB stick, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",6830,"ST",1,"SIMATIC",0.313,1,"6AV63812BN075AX0"]
["6AV6381-2BP07-0AQ0","EPL Royalty for WinCC V7, RC2048 (2048 PowerTags) only valid in connection with Enterprise License agreement, requires EPL Master",7817,"ST",1,"SIMATIC",1.2E-2,1,"6AV63812BP070AQ0"]
["6AV6381-2BP07-4AH0","WinCC system software V7.4 SP1, RC 2048 (2048 Power Tags), Runtime/Configuration software, floating license, SW and license key download Class A, 5 languages (de,en,fr,es,it), executable in Windows 7 Prof/Ent/Ult +SP1 (32 bit)/ 7 Prof/Ent/Ult +SP1 (64 bit)/ 8.1 Prof./Ent (32 bit)/ 8.1 Prof./Ent (64 bit)/ 10 Prof./Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 (64 bit)/ Server 2016 (64 bit) ******************************* E-mail address required for delivery",7817,"ST",1,"SIMATIC",1E-3,1,"6AV63812BP074AH0"]
["6AV6381-2BP07-4AV0","WinCC System SW V7.4 SP1 Asia, RC 2048 (2048 PowerTags), Runtime/configuration software on DVD, floating license, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",8790,"ST",1,"SIMATIC",0.26700000000000002,1,"6AV63812BP074AV0"]
["6AV6381-2BP07-4AX0","WinCC system software V7.4 SP1, RC 2048 (2048 PowerTags), Runtime/configuration software on DVD, floating license, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",8790,"ST",1,"SIMATIC",0.26300000000000001,1,"6AV63812BP074AX0"]
["6AV6381-2BP07-5AH0","WinCC system software V7.5, RC 2048 (2048 PowerTags), Runtime/Configuration software, floating license, SW incl. docu. and license key download, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* E-mail address required for delivery",7817,"ST",1,"SIMATIC",1E-3,1,"6AV63812BP075AH0"]
["6AV6381-2BP07-5AV0","WinCC System SW V7.5 Asia, RC 2048 (2048 PowerTags), Runtime/Configuration software on DVD, floating license, License key on USB stick, Class A, 9 languages (de, en,fr,es,it,zh-s,zh-t,kor,jpn), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",8790,"ST",1,"SIMATIC",0.317,1,"6AV63812BP075AV0"]
["6AV6381-2BP07-5AX0","WinCC system software V7.5, RC 2048 (2048 PowerTags), Runtime/Configuration software on DVD, floating license, License key on USB stick, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",8790,"ST",1,"SIMATIC",0.313,1,"6AV63812BP075AX0"]
["6AV6381-2BQ07-0AQ0","EPL Royalty for WinCC V7, RC65535 (65535 PowerTags) only valid in connection with Enterprise License agreement, requires EPL Master",11235,"ST",1,"SIMATIC",1.2E-2,1,"6AV63812BQ070AQ0"]
["6AV6381-2BQ07-4AH0","WinCC system software V7.4 SP1, RC 65536 (65536 Power Tags), Runtime/Configuration software, floating license, SW and license key download Class A, 5 languages (de,en,fr,es,it), executable in Windows 7 Prof/Ent/Ult +SP1 (32 bit)/ 7 Prof/Ent/Ult +SP1 (64 bit)/ 8.1 Prof./Ent (32 bit)/ 8.1 Prof./Ent (64 bit)/ 10 Prof./Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 (64 bit)/ Server 2016 (64 bit) ******************************* E-mail address required for delivery",11235,"ST",1,"SIMATIC",1E-3,1,"6AV63812BQ074AH0"]
["6AV6381-2BQ07-4AV0","WinCC System SW V7.4 SP1 Asia, RC 65536 (65536 PowerTags), Runtime/configuration software on DVD, floating license, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",12635,"ST",1,"SIMATIC",0.26700000000000002,1,"6AV63812BQ074AV0"]
["6AV6381-2BQ07-4AX0","WinCC system software V7.4 SP1, RC 65536 (65536 PowerTags), Runtime/configuration software on DVD, floating license, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",12635,"ST",1,"SIMATIC",0.26300000000000001,1,"6AV63812BQ074AX0"]
["6AV6381-2BQ07-5AH0","WinCC system software V7.5, RC 65536 (65536 PowerTags), Runtime/Configuration software, floating license, SW incl. docu. and license key download, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* E-mail address required for delivery",11235,"ST",1,"SIMATIC",1E-3,1,"6AV63812BQ075AH0"]
["6AV6381-2BQ07-5AV0","WinCC System SW V7.5 Asia, RC 65536 (65536 PowerTags), Runtime/Configuration software on DVD, floating license, License key on USB stick, Class A, 9 languages (de, en,fr,es,it,zh-s,zh-t,kor,jpn), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",12635,"ST",1,"SIMATIC",0.317,1,"6AV63812BQ075AV0"]
["6AV6381-2BQ07-5AX0","WinCC system software V7.5, RC 65536 (65536 PowerTags), Runtime/Configuration software on DVD, floating license, License key on USB stick, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",12635,"ST",1,"SIMATIC",0.313,1,"6AV63812BQ075AX0"]
["6AV6381-2BS07-0AQ0","EPL Royalty for WinCC V7, RC8192 (8192 PowerTags) only valid in connection with Enterprise License agreement, requires EPL Master",9671,"ST",1,"SIMATIC",1.2E-2,1,"6AV63812BS070AQ0"]
["6AV6381-2BS07-4AH0","WinCC system software V7.4 SP1, RC 8192 (8192 Power Tags), Runtime/Configuration software, floating license, SW and license key download Class A, 5 languages (de,en,fr,es,it), executable in Windows 7 Prof/Ent/Ult +SP1 (32 bit)/ 7 Prof/Ent/Ult +SP1 (64 bit)/ 8.1 Prof./Ent (32 bit)/ 8.1 Prof./Ent (64 bit)/ 10 Prof./Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 (64 bit)/ Server 2016 (64 bit) ******************************* E-mail address required for delivery",9671,"ST",1,"SIMATIC",1E-3,1,"6AV63812BS074AH0"]
["6AV6381-2BS07-4AV0","WinCC System SW V7.4 SP1 Asia, RC 8192 (8192 PowerTags), Runtime/configuration software on DVD, floating license, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",10876,"ST",1,"SIMATIC",0.26700000000000002,1,"6AV63812BS074AV0"]
["6AV6381-2BS07-4AX0","WinCC system software V7.4 SP1, RC 8192 (8192 PowerTags), Runtime/configuration software on DVD, floating license, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",10876,"ST",1,"SIMATIC",0.26300000000000001,1,"6AV63812BS074AX0"]
["6AV6381-2BS07-5AH0","WinCC system software V7.5, RC 8192 (8192 PowerTags), Runtime/Configuration software, floating license, SW incl. docu. and license key download, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* E-mail address required for delivery",9671,"ST",1,"SIMATIC",1E-3,1,"6AV63812BS075AH0"]
["6AV6381-2BS07-5AV0","WinCC System SW V7.5 Asia, RC 8192 (8192 PowerTags), Runtime/Configuration software on DVD, floating license, License key on USB stick, Class A, 9 languages (de, en,fr,es,it,zh-s,zh-t,kor,jpn), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",10876,"ST",1,"SIMATIC",0.317,1,"6AV63812BS075AV0"]
["6AV6381-2BS07-5AX0","WinCC system software V7.5, RC 8192 (8192 PowerTags), Runtime/Configuration software on DVD, floating license, License key on USB stick, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",10876,"ST",1,"SIMATIC",0.313,1,"6AV63812BS075AX0"]
["6AV6381-2BT07-4AH0","WinCC system software V7.4 SP1, RC 102400 (102400 Power Tags), Runtime/Configuration software, floating license, SW and license key download Class A, 5 languages (de,en,fr,es,it), executable in Windows 7 Prof/Ent/Ult +SP1 (32 bit)/ 7 Prof/Ent/Ult +SP1 (64 bit)/ 8.1 Prof./Ent (32 bit)/ 8.1 Prof./Ent (64 bit)/ 10 Prof./Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 (64 bit)/ Server 2016 (64 bit) ******************************* E-mail address required for delivery",12146,"ST",1,"SIMATIC",1E-3,1,"6AV63812BT074AH0"]
["6AV6381-2BT07-4AV0","WinCC System SW V7.4 SP1 Asia, RC 102400 (102400 PowerTags), Runtime/configuration software on DVD, floating license, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",13658,"ST",1,"SIMATIC",0.26700000000000002,1,"6AV63812BT074AV0"]
["6AV6381-2BT07-4AX0","WinCC system software V7.4 SP1, RC 102400 (102400 PowerTags), Runtime/configuration software on DVD, floating license, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",13658,"ST",1,"SIMATIC",0.26300000000000001,1,"6AV63812BT074AX0"]
["6AV6381-2BT07-5AH0","WinCC system software V7.5, RC 102400 (102400 PowerTags), Runtime/Configuration software, floating license, SW incl. docu. and license key download, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* E-mail address required for delivery",12146,"ST",1,"SIMATIC",1E-3,1,"6AV63812BT075AH0"]
["6AV6381-2BT07-5AV0","WinCC System SW V7.5 Asia, RC 102400 (102400 PowerTags), Runtime/Configuration software on DVD, floating license, License key on USB stick, Class A, 9 languages (de, en,fr,es,it,zh-s,zh-t,kor,jpn), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",13659,"ST",1,"SIMATIC",0.317,1,"6AV63812BT075AV0"]
["6AV6381-2BT07-5AX0","WinCC system software V7.5, RC 102400 (102400 PowerTags), Runtime/Configuration software on DVD, floating license, License key on USB stick, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",13659,"ST",1,"SIMATIC",0.313,1,"6AV63812BT075AX0"]
["6AV6381-2BU07-4AH0","WinCC system software V7.4 SP1, RC 153600 (153600 Power Tags), Runtime/Configuration software, floating license, SW and license key download Class A, 5 languages (de,en,fr,es,it), executable in Windows 7 Prof/Ent/Ult +SP1 (32 bit)/ 7 Prof/Ent/Ult +SP1 (64 bit)/ 8.1 Prof./Ent (32 bit)/ 8.1 Prof./Ent (64 bit)/ 10 Prof./Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 (64 bit)/ Server 2016 (64 bit) ******************************* E-mail address required for delivery",12931,"ST",1,"SIMATIC",1E-3,1,"6AV63812BU074AH0"]
["6AV6381-2BU07-4AV0","WinCC System SW V7.4 SP1 Asia, RC 153600 (153600 PowerTags), Runtime/configuration software on DVD, floating license, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",14543,"ST",1,"SIMATIC",0.26700000000000002,1,"6AV63812BU074AV0"]
["6AV6381-2BU07-4AX0","WinCC system software V7.4 SP1, RC 153600 (153600 PowerTags), Runtime/configuration software on DVD, floating license, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",14543,"ST",1,"SIMATIC",0.26300000000000001,1,"6AV63812BU074AX0"]
["6AV6381-2BU07-5AH0","WinCC system software V7.5, RC 153600 (153600 PowerTags), Runtime/Configuration software, floating license, SW incl. docu. and license key download, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* E-mail address required for delivery",12931,"ST",1,"SIMATIC",1E-3,1,"6AV63812BU075AH0"]
["6AV6381-2BU07-5AV0","WinCC System SW V7.5 Asia, RC 153600 (153600 PowerTags), Runtime/Configuration software on DVD, floating license, License key on USB stick, Class A, 9 languages (de, en,fr,es,it,zh-s,zh-t,kor,jpn), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",14543,"ST",1,"SIMATIC",0.317,1,"6AV63812BU075AV0"]
["6AV6381-2BU07-5AX0","WinCC system software V7.5, RC 153600 (153600 PowerTags), Runtime/Configuration software on DVD, floating license, License key on USB stick, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",14543,"ST",1,"SIMATIC",0.313,1,"6AV63812BU075AX0"]
["6AV6381-2BV07-4AH0","WinCC system software V7.4 SP1, RC 262144 (262144 Power Tags), Runtime/Configuration software, floating license, SW and license key download Class A, 5 languages (de,en,fr,es,it), executable in Windows 7 Prof/Ent/Ult +SP1 (32 bit)/ 7 Prof/Ent/Ult +SP1 (64 bit)/ 8.1 Prof./Ent (32 bit)/ 8.1 Prof./Ent (64 bit)/ 10 Prof./Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 (64 bit)/ Server 2016 (64 bit) ******************************* E-mail address required for delivery",17094,"ST",1,"SIMATIC",1E-3,1,"6AV63812BV074AH0"]
["6AV6381-2BV07-4AV0","WinCC System SW V7.4 SP1 Asia, RC 262144 (262144 PowerTags), Runtime/configuration software on DVD, floating license, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",19224,"ST",1,"SIMATIC",0.26700000000000002,1,"6AV63812BV074AV0"]
["6AV6381-2BV07-4AX0","WinCC system software V7.4 SP1, RC 262144 (262144 PowerTags), Runtime/configuration software on DVD, floating license, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",19224,"ST",1,"SIMATIC",0.26300000000000001,1,"6AV63812BV074AX0"]
["6AV6381-2BV07-5AH0","WinCC system software V7.5, RC 262144 (262144 PowerTags), Runtime/Configuration software, floating license, SW incl. docu. and license key download, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* E-mail address required for delivery",17094,"ST",1,"SIMATIC",1E-3,1,"6AV63812BV075AH0"]
["6AV6381-2BV07-5AV0","WinCC System SW V7.5 Asia, RC 262144 (262144 PowerTags), Runtime/Configuration software on DVD, floating license, License key on USB stick, Class A, 9 languages (de, en,fr,es,it,zh-s,zh-t,kor,jpn), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",19224,"ST",1,"SIMATIC",0.317,1,"6AV63812BV075AV0"]
["6AV6381-2BV07-5AX0","WinCC system software V7.5, RC 262144 (262144 PowerTags), Runtime/Configuration software on DVD, floating license, License key on USB stick, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (3x DVD + 1x USB)",19224,"ST",1,"SIMATIC",0.313,1,"6AV63812BV075AX0"]
["6AV6381-2CA07-0AQ0","EPL Royalty for WinCC V7, RT client, only valid in connection with Enterprise License agreement, requires EPL Master",2265,"ST",1,"SIMATIC",1.2999999999999999E-2,1,"6AV63812CA070AQ0"]
["6AV6381-2CA07-4AH0","WinCC RT Client V7.4 SP1 runtime software, single license, SW and license key download, Class A, 5 languages (de,en,fr,es,it), executable in Windows 7 Prof/Ent/Ult +SP1 (32 bit)/ 7 Prof/Ent/Ult +SP1 (64 bit)/ 8.1 Prof./Ent (32 bit)/ 8.1 Prof./Ent (64 bit)/ 10 Prof./Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 (64 bit)/ Server 2016 (64 bit) ******************************* E-mail address required for delivery",2265,"ST",1,"SIMATIC",1E-3,1,"6AV63812CA074AH0"]
["6AV6381-2CA07-4AK3","SIMATIC WinCC RT Client upgrade from V7.X to V7.4 SP1, for WinCC RT Clients w/o RT 128, runtime software, single license, SW and License Key Download ******************************* E-mail address required for delivery",563,"ST",1,"SIMATIC",1E-3,1,"6AV63812CA074AK3"]
["6AV6381-2CA07-4AV0","WinCC RT Client V7.4 SP1 Asia runtime software, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 9 languages (de,en,fr,es,it, zh-s,zh-t,kor,jpn), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",2548,"ST",1,"SIMATIC",0.216,1,"6AV63812CA074AV0"]
["6AV6381-2CA07-4AV3","SIMATIC WinCC RT CL Upgrade Asia from V7.X to V7.4 SP1 for WinCC RT Clients w/o RT 128, runtime software on DVD, single license, license key on USB flash drive ******************************* Content: Set (2x DVD + 1x USB)",634,"ST",1,"SIMATIC",0.216,1,"6AV63812CA074AV3"]
["6AV6381-2CA07-4AX0","WinCC RT Client V7.4 SP1 runtime software, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",2548,"ST",1,"SIMATIC",0.21199999999999999,1,"6AV63812CA074AX0"]
["6AV6381-2CA07-4AX3","SIMATIC WinCC RT client upgrade from V7.X to V7.4 SP1 for WinCC RT Clients w/o RT 128, runtime software on DVD, single license, license key on USB flash drive ******************************* Content: Set (2x DVD + 1x USB)",634,"ST",1,"SIMATIC",0.21199999999999999,1,"6AV63812CA074AX3"]
["6AV6381-2CA07-5AH0","WinCC system software V7.5, WinCC RT Client V7.5 runtime software, single license, SW incl. documentation and license key download, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* E-mail address required for delivery",2265,"ST",1,"SIMATIC",1E-3,1,"6AV63812CA075AH0"]
["6AV6381-2CA07-5AK3","SIMATIC WinCC RT client upgrade from V7.2/7.3 to V7.5 for WinCC RT clients w/o RT 128, runtime software, single license, SW and license key download ******************************* E-mail address required for delivery",563,"ST",1,"SIMATIC",1E-3,1,"6AV63812CA075AK3"]
["6AV6381-2CA07-5AK4","SIMATIC WinCC RT client upgrade from V7.4 to V7.5 for WinCC RT clients w/o RT 128, runtime software, single license, SW and license key download ******************************* E-mail address required for delivery",375,"ST",1,"SIMATIC",1E-3,1,"6AV63812CA075AK4"]
["6AV6381-2CA07-5AV0","WinCC System SW V7.5 Asia, WinCC RT Client V7.5 Asia runtime software, single license, SW and documentation on DVD, License key on USB stick, Class A, 9 languages (de, en,fr,es,it,zh-s,zh-t,kor,jpn), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (2x DVD + 1x USB)",2549,"ST",1,"SIMATIC",0.26600000000000001,1,"6AV63812CA075AV0"]
["6AV6381-2CA07-5AV3","SIMATIC WinCC RT CL Upgrade Asia from V7.2/7.3 to V7.5 for WinCC RT Clients w/o RT 128, runtime software on DVD, single license, license key on USB flash drive ******************************* Content: Set (2x DVD + 1x USB)",635,"ST",1,"SIMATIC",0.26600000000000001,1,"6AV63812CA075AV3"]
["6AV6381-2CA07-5AV4","SIMATIC WinCC RT CL Upgrade Asia from V7.4 to V7.5 for WinCC RT Clients w/o RT 128, runtime software on DVD, single license, license key on USB flash drive ******************************* Content: Set (2x DVD + 1x USB)",423,"ST",1,"SIMATIC",0.26600000000000001,1,"6AV63812CA075AV4"]
["6AV6381-2CA07-5AX0","WinCC system software V7.5, WinCC RT Client V7.5 runtime software, single license, SW and documentation on DVD, License key on USB stick, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (2x DVD + 1x USB)",2549,"ST",1,"SIMATIC",0.26200000000000001,1,"6AV63812CA075AX0"]
["6AV6381-2CA07-5AX3","SIMATIC WinCC RT client upgrade from V7.2/7.3 to V7.5 for WinCC RT clients w/o RT 128, runtime software on DVD, single license, license key on USB flash drive ******************************* Content: Set (2x DVD + 1x USB)",635,"ST",1,"SIMATIC",0.26200000000000001,1,"6AV63812CA075AX3"]
["6AV6381-2CA07-5AX4","SIMATIC WinCC RT client upgrade from V7.4 to V7.5 for WinCC RT Clients w/o RT 128, runtime software on DVD, single license, license key on USB flash drive ******************************* Content: Set (2x DVD + 1x USB)",423,"ST",1,"SIMATIC",0.26200000000000001,1,"6AV63812CA075AX4"]
["6AV6381-2CB07-4AH0","WinCC RC Client V7.4 SP1 Runtime/Configuration software, SW and license key download, Class A, 5 languages (de,en,fr,es,it), executable in Windows 7 Prof/Ent/Ult +SP1 (32 bit)/ 7 Prof/Ent/Ult +SP1 (64 bit)/ 8.1 Prof./Ent (32 bit)/ 8.1 Prof./Ent (64 bit)/ 10 Prof./Ent (64 bit)/ Server 2008 R2+SP1 (64 bit)/ Server 2012 R2 (64 bit)/ Server 2016 (64 bit) ******************************* E-mail address required for delivery",3395,"ST",1,"SIMATIC",1E-3,1,"6AV63812CB074AH0"]
["6AV6381-2CB07-4AK3","SIMATIC WinCC RC Client upgrade from V7.X to V7.4 SP1, for WinCC RC Clients w/o RC 128, runtime/configuration software, single license, SW and License Key Download ******************************* E-mail address required for delivery",945,"ST",1,"SIMATIC",1E-3,1,"6AV63812CB074AK3"]
["6AV6381-2CB07-4AV0","WinCC RC Client V7.4 SP1 Asia Runtime/configuration software on DVD, floating license, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",3818,"ST",1,"SIMATIC",0.216,1,"6AV63812CB074AV0"]
["6AV6381-2CB07-4AV3","SIMATIC WinCC RC CL Upgrade Asia from V7.X to V7.4 SP1 for WinCC RC Clients w/o RC128, Runtime/configuration software on DVD, single license, license key on USB flash drive ******************************* Content: Set (2x DVD + 1x USB)",1063,"ST",1,"SIMATIC",0.216,1,"6AV63812CB074AV3"]
["6AV6381-2CB07-4AX0","WinCC RC Client V7.4 SP1 Runtime/configuration software on DVD, floating license, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows 7 Prof/Ent/Ult +SP1 (32-bit)/ 7 Prof/Ent/Ult +SP1 (64-bit)/ 8.1 Prof./Ent (32-bit)/ 8.1 Prof./Ent (64-bit)/ 10 Prof./Ent (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ******************************* Content: Set (2x DVD + 1x USB)",3818,"ST",1,"SIMATIC",0.21199999999999999,1,"6AV63812CB074AX0"]
["6AV6381-2CB07-4AX3","SIMATIC WinCC RC client upgrade from V7.X to V7.4 SP1 for WinCC RC Clients w/o RC128, Runtime/configuration software on DVD, single license, license key on USB flash drive ******************************* Content: Set (2x DVD + 1x USB)",1063,"ST",1,"SIMATIC",0.21199999999999999,1,"6AV63812CB074AX3"]
["6AV6381-2CB07-5AH0","WinCC system software V7.5, WinCC RC Client V7.5 Runtime/Configuration software, floating license, SW incl. docu. and license key download, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* E-mail address required for delivery",3395,"ST",1,"SIMATIC",1E-3,1,"6AV63812CB075AH0"]
["6AV6381-2CB07-5AK3","SIMATIC WinCC RC client upgrade from V7.2/7.3 to V7.5 for WinCC RC clients w/o RC128, runtime/configuration software, Single license, SW and license key download ******************************* E-mail address required for delivery",945,"ST",1,"SIMATIC",1E-3,1,"6AV63812CB075AK3"]
["6AV6381-2CB07-5AK4","SIMATIC WinCC RC client upgrade from V7.4 to V7.5 for WinCC RC clients w/o RC128, runtime/configuration software, Single license, SW and license key download ******************************* E-mail address required for delivery",668,"ST",1,"SIMATIC",1E-3,1,"6AV63812CB075AK4"]
["6AV6381-2CB07-5AV0","WinCC System SW V7.5 Asia, WinCC RC Client V7.5 Asia Runtime/Configuration software on DVD, floating license, License key on USB stick, Class A, 9 languages (de, en,fr,es,it,zh-s,zh-t,kor,jpn), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (2x DVD + 1x USB)",3818,"ST",1,"SIMATIC",0.26600000000000001,1,"6AV63812CB075AV0"]
["6AV6381-2CB07-5AV3","SIMATIC WinCC RC CL Upgrade Asia from V7.2/7.3 to V7.5 for WinCC RC Clients w/o RC128, Runtime/configuration software on DVD, single license, license key on USB flash drive ******************************* Content: Set (2x DVD + 1x USB)",1064,"ST",1,"SIMATIC",0.26600000000000001,1,"6AV63812CB075AV3"]
["6AV6381-2CB07-5AV4","SIMATIC WinCC RC CL Upgrade Asia from V7.4 to V7.5 for WinCC RC Clients w/o RC128, Runtime/configuration software on DVD, single license, license key on USB flash drive ******************************* Content: Set (2x DVD + 1x USB)",751,"ST",1,"SIMATIC",0.26600000000000001,1,"6AV63812CB075AV4"]
["6AV6381-2CB07-5AX0","WinCC system software V7.5, WinCC RC Client V7.5 Runtime/Configuration software on DVD, floating license, License key on USB stick, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 ******************************* Content: set (2x DVD + 1x USB)",3818,"ST",1,"SIMATIC",0.26200000000000001,1,"6AV63812CB075AX0"]
["6AV6381-2CB07-5AX3","SIMATIC WinCC RC client upgrade from V7.2/7.3 to V7.5 for WinCC RC Clients w/o RC128, Runtime/configuration software on DVD, single license, license key on USB flash drive ******************************* Content: Set (2x DVD + 1x USB)",1064,"ST",1,"SIMATIC",0.26200000000000001,1,"6AV63812CB075AX3"]
["6AV6381-2CB07-5AX4","SIMATIC WinCC RC client upgrade from V7.4 to V7.5 for WinCC RC Clients w/o RC128, Runtime/configuration software on DVD, single license, license key on USB flash drive ******************************* Content: Set (2x DVD + 1x USB)",751,"ST",1,"SIMATIC",0.26200000000000001,1,"6AV63812CB075AX4"]
["6AV6381-2DC07-4AX0","WinCC system software V7.4 SP1, RT 500000 (500000 PowerTags), runtime software, single license, SW and documentation on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows as RT 128 (6AV6381-2BC07-4AX0) The license is a customer-specific solution and not released/ system-tested as standard. Support by the standard hotline is not possible. Overall responsibility for functionality and performance lies with the user ******************************* Content: Set (2x DVD + 1x USB)",38819,"ST",1,"SIMATIC",0.252,1,"6AV63812DC074AX0"]
["6AV6381-2DC07-5AH0","WinCC system software V7.5, RT 500000 (500000 PowerTags), runtime software, single license, SW incl. documentation and license key download, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 Special license for customer- specific solution. Not system- tested/released No hotline support Overall responsibility for Functionality and performance lies with the customer. ******************************* E-mail address required for delivery",38058,"ST",1,"SIMATIC",1E-3,1,"6AV63812DC075AH0"]
["6AV6381-2DC07-5AX0","WinCC system software V7.5, RT 500000 (500000 PowerTags), runtime software, single license, SW and documentation on DVD, License key on USB stick, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 Special license for customer- specific solution. Not system- tested/released No hotline support Overall responsibility for Functionality and performance lies with the customer. ******************************* Content: set (3x DVD + 1x USB)",38819,"ST",1,"SIMATIC",0.30199999999999999,1,"6AV63812DC075AX0"]
["6AV6381-2DM07-4AX0","WinCC system software V7.4 SP1, RC 500000 (500000 PowerTags), Runtime/configuration software on DVD, floating license, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Executable in Windows as RC128 (6AV6381-2BM07-4AX0) The license is a customer-specific solution and not released/ system-tested as standard. Support by the standard hotline is not possible. Overall responsibility for functionality and performance lies with the user ******************************* Content: Set (2x DVD + 1x USB)",38819,"ST",1,"SIMATIC",0.252,1,"6AV63812DM074AX0"]
["6AV6381-2DM07-5AH0","WinCC system software V7.5, RC 500000 (500000 PowerTags), Runtime/Configuration software, floating license, SW incl. docu. and license key download, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 Special license for customer- specific solution. Not system- tested/released No hotline support Overall responsibility for Functionality and performance lies with the customer. ******************************* E-mail address required for delivery",38058,"ST",1,"SIMATIC",1E-3,1,"6AV63812DM075AH0"]
["6AV6381-2DM07-5AX0","WinCC system software V7.5, RC 500000 (500000 PowerTags), Runtime/Configuration software on DVD, floating license, License key on USB stick, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109759993 Special license for customer- specific solution. Not system- tested/released No hotline support Overall responsibility for Functionality and performance lies with the customer. ******************************* Content: set (3x DVD + 1x USB)",38819,"ST",1,"SIMATIC",0.30199999999999999,1,"6AV63812DM075AX0"]
["6AV6381-2EA07-2AV0","SIMATIC WinCC Asia License key USB hardlock ******************************* Content: 1x USB",97.3,"ST",1,"SIMATIC",0.216,1,"6AV63812EA072AV0"]
["6AV6382-2AA07-4AX0","WinCC package for SIMATIC IPC, consisting of: WinCC RT Client, V7.4; Supply only if the same number of SIMATIC IPCs is ordered on the same order slip ******************************* Content: 6AV6381-2CA07-4AX0",1783,"ST",1,"SIMATIC",0.2,1,"6AV63822AA074AX0"]
["6AV6382-2AA07-5AV0","WinCC package for SIMATIC IPC, consists of: WinCC RT Client, V7.5 Asia; Supply only if the same number of SIMATIC IPCs is ordered on the same order slip ******************************* Content: 6AV6381-2CA07-5AV0",1784,"ST",1,"SIMATIC",0.2,1,"6AV63822AA075AV0"]
["6AV6382-2AA07-5AX0","WinCC package for SIMATIC IPC, consists of: WinCC RT Client, V7.5; Supply only if the same number of SIMATIC IPCs is ordered on the same order slip ******************************* Content: 6AV6381-2CA07-5AX0",1784,"ST",1,"SIMATIC",0.2,1,"6AV63822AA075AX0"]
["6AV6382-2CA07-4AX0","WinCC package for SIMATIC IPC, consisting of: WinCC RT 128, V7.4; Supply only if the same number of SIMATIC IPCs is ordered on the same order slip ******************************* Content: 6AV6381-2BC07-4AX0",1872,"ST",1,"SIMATIC",0.2,1,"6AV63822CA074AX0"]
["6AV6382-2CA07-5AV0","WinCC package for SIMATIC IPC, consists of: WinCC RT 128, V7.5 Asia; Supply only if the same number of SIMATIC IPCs is ordered on the same order slip ******************************* Content: 6AV6381-2BC07-5AV0",1873,"ST",1,"SIMATIC",0.2,1,"6AV63822CA075AV0"]
["6AV6382-2CA07-5AX0","WinCC package for SIMATIC IPC, consists of: WinCC RT 128, V7.5; Supply only if the same number of SIMATIC IPCs is ordered on the same order slip ******************************* Content: 6AV6381-2BC07-5AX0",1873,"ST",1,"SIMATIC",0.2,1,"6AV63822CA075AX0"]
["6AV6382-2DA07-4AX0","WinCC package for SIMATIC IPC, consisting of: WinCC RT 512, V7.4; Supply only if the same number of SIMATIC IPCs is ordered on the same order slip ******************************* Content: 6AV6381-2BD07-4AX0",3075,"ST",1,"SIMATIC",0.2,1,"6AV63822DA074AX0"]
["6AV6382-2DA07-5AV0","WinCC package for SIMATIC IPC, consists of: WinCC RT 512, V7.5 Asia; Supply only if the same number of SIMATIC IPCs is ordered on the same order slip ******************************* Content: 6AV6381-2BD07-5AV0",3075,"ST",1,"SIMATIC",0.2,1,"6AV63822DA075AV0"]
["6AV6382-2DA07-5AX0","WinCC package for SIMATIC IPC, consists of: WinCC RT 512, V7.5; Supply only if the same number of SIMATIC IPCs is ordered on the same order slip ******************************* Content: 6AV6381-2BD07-5AX0",3075,"ST",1,"SIMATIC",0.2,1,"6AV63822DA075AX0"]
["6AV6382-2EA07-2AX0","SIMATIC WinCC Package for SIMATIC IPC, Consisting of: WinCC RT 2048, V7.2 Connection via onboard Interfaces Supply only if the same number of SIMATIC IPCs is ordered on the same order slip",3910,"ST",1,"SIMATIC",0.3,1,"6AV63822EA072AX0"]
["6AV6382-2EA07-4AX0","WinCC package for SIMATIC IPC, consisting of: WinCC RT 2048, V7.4; Supply only if the same number of SIMATIC IPCs is ordered on the same order slip ******************************* Content: 6AV6381-2BE07-4AX0",3795,"ST",1,"SIMATIC",0.2,1,"6AV63822EA074AX0"]
["6AV6382-2EA07-5AV0","WinCC package for SIMATIC IPC, consists of: WinCC RT 2048, V7.5 Asia; Supply only if the same number of SIMATIC IPCs is ordered on the same order slip ******************************* Content: 6AV6381-2BE07-5AV0",3795,"ST",1,"SIMATIC",0.2,1,"6AV63822EA075AV0"]
["6AV6382-2EA07-5AX0","WinCC package for SIMATIC IPC, consists of: WinCC RT 2048, V7.5; Supply only if the same number of SIMATIC IPCs is ordered on the same order slip ******************************* Content: 6AV6381-2BE07-5AX0",3795,"ST",1,"SIMATIC",0.2,1,"6AV63822EA075AX0"]
["6AV6382-2FA07-4AX0","WinCC package for SIMATIC IPC, consisting of: WinCC RT 65536, V7.4; Supply only if the same number of SIMATIC IPCs is ordered on the same order slip ******************************* Content: 6AV6381-2BF07-4AX0",5952,"ST",1,"SIMATIC",0.2,1,"6AV63822FA074AX0"]
["6AV6382-2FA07-5AV0","WinCC package for SIMATIC IPC, consists of: WinCC RT 65536, V7.5 Asia; Supply only if the same number of SIMATIC IPCs is ordered on the same order slip ******************************* Content: 6AV6381-2BF07-5AV0",5952,"ST",1,"SIMATIC",0.2,1,"6AV63822FA075AV0"]
["6AV6382-2FA07-5AX0","WinCC package for SIMATIC IPC, consists of: WinCC RT 65536, V7.5; Supply only if the same number of SIMATIC IPCs is ordered on the same order slip ******************************* Content: 6AV6381-2BF07-5AX0",5952,"ST",1,"SIMATIC",0.2,1,"6AV63822FA075AX0"]
["6AV6382-2HA07-4AX0","WinCC package for SIMATIC IPC, consisting of: WinCC RT 8192, V7.4; Supply only if the same number of SIMATIC IPCs is ordered on the same order slip ******************************* Content: 6AV6381-2BH07-4AX0",4874,"ST",1,"SIMATIC",0.2,1,"6AV63822HA074AX0"]
["6AV6382-2HA07-5AV0","WinCC package for SIMATIC IPC, consists of: WinCC RT 8192, V7.5 Asia; Supply only if the same number of SIMATIC IPCs is ordered on the same order slip ******************************* Content: 6AV6381-2BH07-5AV0",4874,"ST",1,"SIMATIC",0.2,1,"6AV63822HA075AV0"]
["6AV6382-2HA07-5AX0","WinCC package for SIMATIC IPC, consists of: WinCC RT 8192, V7.5; Supply only if the same number of SIMATIC IPCs is ordered on the same order slip ******************************* Content: 6AV6381-2BH07-5AX0",4874,"ST",1,"SIMATIC",0.2,1,"6AV63822HA075AX0"]
["6AV6387-1BC07-2AF3","FL migration package RT, WinCC V7.5 RT 128 (128 PowerTags), Runtime, on DVD, single license, 5 languages (de,en,fr,es,it). This is a special offer and is valid if you replace the previously used product FactoryLink with the product WinCC V7.5. By purchasing this product you obligate yourself to replace the previously used product FactoryLink (after a transitional period of 12 months after receiving this product) with WinCC V7.5 and to no longer use the FactoryLink license. Only customer with SUS contract",1340,"ST",1,"SIMATIC",0.3,1,"6AV63871BC072AF3"]
["6AV6387-1BD07-2AF3","FL migration package RT, WinCC V7.5 RT 512 (512 PowerTags), Runtime, on DVD, single license, 5 languages (de,en,fr,es,it). This is a special offer and is valid if you replace the previously used product FactoryLink with the product WinCC V7.5. By purchasing this product you obligate yourself to replace the previously used product FactoryLink (after a transitional period of 12 months after receiving this product) with WinCC V7.5 and to no longer use the FactoryLink license. Only customer with SUS contract",2058,"ST",1,"SIMATIC",0.3,1,"6AV63871BD072AF3"]
["6AV6387-1BE07-2AF3","FL migration package RT, WinCC V7.5 RT 2048 (2048 PowerTags), Runtime, on DVD, single license, 5 languages (de,en,fr,es,it). This is a special offer and is valid if you replace the previously used product FactoryLink with the product WinCC V7.5. By purchasing this product you obligate yourself to replace the previously used product FactoryLink (after a transitional period of 12 months after receiving this product) with WinCC V7.5 and to no longer use the FactoryLink license. Only customer with SUS contract",2530,"ST",1,"SIMATIC",0.3,1,"6AV63871BE072AF3"]
["6AV6387-1BF07-2AF3","FL migration package RT, WinCC V7.5 RT 65536 (65536 PowerTags), Runtime, on DVD, single license, 5 languages (de,en,fr,es,it). This is a special offer and is valid if you replace the previously used product FactoryLink with the product WinCC V7.5. By purchasing this product you obligate yourself to replace the previously used product FactoryLink (after a transitional period of 12 months after receiving this product) with WinCC V7.5 and to no longer use the FactoryLink license. Only customer with SUS contract",3733,"ST",1,"SIMATIC",0.3,1,"6AV63871BF072AF3"]
["6AV6387-1BH07-2AF3","FL migration package RT, WinCC V7.5 RT 8192 (8192 PowerTags), Runtime, on DVD, single license, 5 languages (de,en,fr,es,it), This is a special offer and is valid if you replace the previously used product FactoryLink with the product WinCC V7.5. By purchasing this product you obligate yourself to replace the previously used product FactoryLink (after a transitional period of 12 months after receiving this product) with WinCC V7.5 and to no longer use the FactoryLink license. Only customer with SUS contract",3039,"ST",1,"SIMATIC",0.3,1,"6AV63871BH072AF3"]
["6AV6387-1BL07-2AF3","FL migration package RT, WinCC V7.5 RT 262144 (262144 PowerTags), Runtime, on DVD, single license, 5 languages (de,en,fr,es,it). This is a special offer and is valid if you replace the previously used product FactoryLink with the product WinCC V7.5. By purchasing this product you obligate yourself to replace the previously used product FactoryLink (after a transitional period of 12 months after receiving this product) with WinCC V7.5 and to no longer use the FactoryLink license. Only customer with SUS contract",9361,"ST",1,"SIMATIC",0.3,1,"6AV63871BL072AF3"]
["6AV6387-1BM07-2AF3","FL migration package RC, WinCC V7.5 RC 128 (128 PowerTags), Runtime, on DVD, single license, 5 languages (de,en,fr,es,it). This is a special offer and is valid if you replace the previously used product FactoryLink with the product WinCC V7.5. By purchasing this product you obligate yourself to replace the previously used product FactoryLink (after a transitional period of 12 months after receiving this product) with WinCC V7.5 and to no longer use the FactoryLink license. Only customer with SUS contract",2009,"ST",1,"SIMATIC",0.3,1,"6AV63871BM072AF3"]
["6AV6387-1BN07-2AF3","FL migration package RC, WinCC V7.5 RC 512 (512 PowerTags), Runtime, on DVD, single license, 5 languages (de,en,fr,es,it) This is a special offer and is valid if you replace the previously used product FactoryLink with the product WinCC V7.5. By purchasing this product you obligate yourself to replace the previously used product FactoryLink (after a transitional period of 12 months after receiving this product) with WinCC V7.5 and to no longer use the FactoryLink license. Only customer with SUS contract",3417,"ST",1,"SIMATIC",0.3,1,"6AV63871BN072AF3"]
["6AV6387-1BP07-2AF3","FL migration package RC, WinCC V7.5 RC 2048 (2048 PowerTags), Runtime, on DVD, single license, 5 languages (de,en,fr,es,it) This is a special offer and is valid if you replace the previously used product FactoryLink with the product WinCC V7.5. By purchasing this product you obligate yourself to replace the previously used product FactoryLink (after a transitional period of 12 months after receiving this product) with WinCC V7.5 and to no longer use the FactoryLink license. Only customer with SUS contract",4395,"ST",1,"SIMATIC",0.3,1,"6AV63871BP072AF3"]
["6AV6387-1BQ07-2AF3","FL migration package RC, WinCC V7.5 RC 65536 (65536 PowerTags), Runtime, on DVD, single license, 5 languages (de,en,fr,es,it) This is a special offer and is valid if you replace the previously used product FactoryLink with the product WinCC V7.5. By purchasing this product you obligate yourself to replace the previously used product FactoryLink (after a transitional period of 12 months after receiving this product) with WinCC V7.5 and to no longer use the FactoryLink license. Only customer with SUS contract",6318,"ST",1,"SIMATIC",0.3,1,"6AV63871BQ072AF3"]
["6AV6387-1BS07-2AF3","FL migration package RC, WinCC V7.5 RC 8192 (8192 PowerTags), Runtime, on DVD, single license, 5 languages (de,en,fr,es,it). This is a special offer and is valid if you replace the previously used product FactoryLink with the product WinCC V7.5. By purchasing this product you obligate yourself to replace the previously used product FactoryLink (after a transitional period of 12 months after receiving this product) with WinCC V7.5 and to no longer use the FactoryLink license. Only customer with SUS contract",5437,"ST",1,"SIMATIC",0.3,1,"6AV63871BS072AF3"]
["6AV6387-1BV07-2AF3","FL migration package RC, WinCC V7.5 RC 262144 (262144 PowerTags), Runtime, on DVD, single license, 5 languages (de,en,fr,es,it). This is a special offer and is valid if you replace the previously used product FactoryLink with the product WinCC V7.5. By purchasing this product you obligate yourself to replace the previously used product FactoryLink (after a transitional period of 12 months after receiving this product) with WinCC V7.5 and to no longer use the FactoryLink license. Only customer with SUS contract",9616,"ST",1,"SIMATIC",0.3,1,"6AV63871BV072AF3"]
["6AV6387-1CA07-4AF3","FL migration package RT, WinCC V7.5, RT client, software on DVD, single license This is a special offer and is valid if you replace the previously used product FactoryLink with the product WinCC V7.5. By purchasing this product you obligate yourself to replace the previously used product FactoryLink (following a transitional period of 12 months after receiving this product) with WinCC V7.5 and to no longer use the FactoryLink license. For customers with SUS contract ******************************* Content: 6AV6381-2CA07-5AX0",1312,"ST",1,"SIMATIC",0.2,1,"6AV63871CA074AF3"]
["6AV6574-1AA00-2BX0","Service set for 12\" devices, MP 370 12\" Key, TP37, Further information, Quantity and content: see technical data",154,"ST",1,"SIMATIC",0.623,1,"6AV65741AA002BX0"]
["6AV6574-1AA00-4AG0","Service pack for TP 170 6\" with stainless steel front",72.099999999999994,"ST",1,"SIMATIC",1E-3,1,"6AV65741AA004AG0"]
["6AV6574-1AA00-4AX0","Service set 6β€\u009d devices, type 1 Service set for TP 070, TP 170A/B, OP 170B, TP 170micro, OP 270 6\", TP 270 6\", MP 270B 6\" Touch Further information, Quantity and content: see technical data",110,"ST",1,"SIMATIC",7.4999999999999997E-2,1,"6AV65741AA004AX0"]
["6AV6574-1AA00-4BG0","Service pack for TP 270 10\" Touch with stainless steel front",70.699999999999989,"ST",1,"SIMATIC",1E-3,1,"6AV65741AA004BG0"]
["6AV6574-1AA00-4CG0","Service pack for MP 370 15\" Touch with with stainless steel front",118,"ST",1,"SIMATIC",1E-3,1,"6AV65741AA004CG0"]
["6AV6574-1AA04-4AA0","Service set mobile panel Service set for Further information, Quantity and content: see technical data",110,"ST",1,"SIMATIC",7.1999999999999995E-2,1,"6AV65741AA044AA0"]
["6AV6574-1AB00-2BA0","Labeling strips, MP37x Key Labeling strips for Further information, Quantity and content: see technical data",44.1,"PAK",1,"SIMATIC",5.5E-2,1,"6AV65741AB002BA0"]
["6AV6574-1AB04-4AA0","Protective cover for labeling strips Protective cover for Mobile Panel 170, Mobile Panel 177 Further information, Quantity and content: see technical data",65.099999999999994,"PAK",1,"SIMATIC",7.4999999999999997E-2,1,"6AV65741AB044AA0"]
["6AV6574-1AD00-4AX0","Protective film 6\" touch devices, type 1, for TP 070, TP 170MICRO, TP 170A/B, C7-635 Touch Quantity: see technical data",65.099999999999994,"PAK",1,"SIMATIC",0.08,1,"6AV65741AD004AX0"]
["6AV6574-1AD00-4CX0","Protective film 10\" to 12\" touch devices for TP 270 10\", MP 270B 10\", MP 370 12\" Touch, MP 377 12\" Touch, C7-636 Touch Quantity: see technical data",126,"PAK",1,"SIMATIC",0.34300000000000003,1,"6AV65741AD004CX0"]
["6AV6574-1AD00-4DX0","Protective film 6\" touch devices, type 2, for TP 270 6\", TP 277 6\", MP 177 6\" Touch, MP 270B 6\" Touch Quantity: see technical data",76.699999999999989,"PAK",1,"SIMATIC",0.115,1,"6AV65741AD004DX0"]
["6AV6574-1AD00-4EX0","Protective film 15\" touch devices for MP 370 15\" Touch, TP 1500 Basic, MP 377 15\" Touch and Thin Client 15\" Quantity: see technical data",110,"PAK",1,"SIMATIC",0.434,1,"6AV65741AD004EX0"]
["6AV6574-1AD04-4AA0","Protective film 6\" touch devices, type 10, for Mobile Panel 170, Mobile Panel 177 Quantity: see technical data",65.099999999999994,"PAK",1,"SIMATIC",0.08,1,"6AV65741AD044AA0"]
["6AV6574-1AE00-4AX0","Protective cover for TP 070, TP 170A, TP 170B, TP 170MICRO, TP 177micro, TP 177A, TP 177B, TP 270 6\", TP 277 6\", MP 270 6\" Touch Quantity: see technical data",94.5,"ST",1,"SIMATIC",0.47499999999999998,1,"6AV65741AE004AX0"]
["6AV6574-1AF04-4AA0","Wall holder, Type 10 fΓΌr Mobile Panel 170, Mobile Panel 177, Mobile Panel 277, Mobile Panel 277 IWLAN, Mobile Panel 277F IWLAN, Mobile Client900, without fixing parts Further information, Quantity and content: see technical data",98.7,"ST",1,"SIMATIC",0.81699999999999995,1,"6AV65741AF044AA0"]
["6AV6574-1AG04-4AA0","Spare key type 10 for key-operated switches Mobile Panel Further information, Quantity and content: see technical data",242,"PAK",1,"SIMATIC",5.3999999999999999E-2,1,"6AV65741AG044AA0"]
["6AV6574-2AC00-2AA1","SIMATIC HMI CF memory card, 512 MB, for for HMI devices and IPCs with corresponding slot Further information, Quantity and content: see technical data",110,"ST",1,"SIMATIC",1.7000000000000001E-2,1,"6AV65742AC002AA1"]
["6AV6611-0AA01-0AQ0","EPL Royalty for WinCC flexible Compact, only valid in connection with enterprise license agreement, requires EPL Master ******************************* E-mail address required for delivery",323,"ST",1,"SIMATIC",1E-3,1,"6AV66110AA010AQ0"]
["6AV6611-0AA01-3UE3","WinCC flexible 2008 Compact Unlock Copy License (UCL), MLK update for 64-bit operating systems only valid in connection with Unlock Copy License agreement",39.700000000000003,"ST",1,"SIMATIC",0.17399999999999999,1,"6AV66110AA013UE3"]
["6AV6611-0AA51-3CA5","WinCC flexible 2008 Compact engineering software,Floating License license key on USB flash drive, SW and documentation on DVD in de/en/fr/it/sp/zh-s/zh-t/kor/ja p executable in Windows 7 Prof/Ultimate/Enterprise(32/64) Windows 10 Pro/Enterprise (64), for configuration of SIMATIC Panels up to 170 series and Basic Panels ******************************* Content: Set (1x DVD + 1x USB)",342,"ST",1,"SIMATIC",0.21099999999999999,1,"6AV66110AA513CA5"]
["6AV6611-0AA51-3CE5","WinCC flexible 2008 Compact, upgrade for WinCC flexible 2004/2005/2007 Compact, incl. Change Control, engineering software,Floating License license key on USB flash drive, SW and documentation on DVD, de/en/fr/it/sp/zh-s/zh-t/kor/ja p, executable in Windows 7 Prof/Ultimate/Enterprise(32/64) Windows 10 Pro/Enterprise (64) ******************************* Content: Set (1x DVD + 1x USB)",138,"ST",1,"SIMATIC",0.21099999999999999,1,"6AV66110AA513CE5"]
["6AV6611-0AA51-3CH5","WinCC flexible 2008 Compact Engineering software,Floating License Software and License key download, d/e/f/i/s/chs/cht/kor/jap Executable under Windows 7 Prof/Ultimate/Enterprise(32/64) Windows 10 Prof/Enterprise (64), for configuration of SIMATIC Panels to 170 series and Basic Panels ******************************* E-mail address required for delivery",294,"ST",1,"SIMATIC",1E-3,1,"6AV66110AA513CH5"]
["6AV6611-0AA51-3CK5","WinCC flexible 2008 Compact, Upgrade for WinCC flexible 2004/2005/2007 Compact, incl. Change Control, Engineering SW,Floating License Software and License key download, d/e/f/i/s/chs/cht/kor/jap, Executable under Windows 7 Prof/Ultimate/Enterprise(32/64) Windows 10 Prof/Enterprise (64) ******************************* E-mail address required for delivery",118,"ST",1,"SIMATIC",1E-3,1,"6AV66110AA513CK5"]
["6AV6611-8AA00-0AR0","EPL-Maintenance WinCC flexible compact (EPL=Enterprise License) Payment for maintenance of a Royalty for 12 months, only valid in connection with Enterprise License contract, requires EPL Master",97.1,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV66118AA000AR0"]
["6AV6612-0AA00-0AL0","SIMATIC WinCC Comfort Software Update Service within the framework of this contract, you will receive for one year all up-to-date software versions. the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software",155,"ST",1,"SIMATIC",0.1,1,"6AV66120AA000AL0"]
["6AV6612-0AA00-0AM0","SIMATIC WinCC Comfort Software Update Service Compact for multiple orders on one position, these deliveries are grouped. Minimum order quantity: 3 units within the framework of this contract, you will receive for one year all up-to-date software versions. the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software",155,"ST",1,"SIMATIC",1.2E-2,1,"6AV66120AA000AM0"]
["6AV6612-0AA00-0AY0","SIMATIC WinCC Comfort SUS (download) Software Update Service, within the framework of this contract, you will receive for one year all up-to-date software versions, the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software ******************************* E-mail address required for delivery",144,"ST",1,"SIMATIC",1E-3,1,"6AV66120AA000AY0"]
["6AV6612-0AA00-0UL0","SIMATIC WinCC Comfort Unlock Copy License (UCL) Software Update Service, Automatic subsequent deliveries of upgrades and service packs for one year with automatic extension, requires current software version, only valid in connection with Unlock Copy License agreement Minimum ordering quantity 20 units",131,"ST",1,"SIMATIC",1.2E-2,1,"6AV66120AA000UL0"]
["6AV6612-0AA00-0UY0","SIMATIC WinCC Comfort SUS (UCL download) Software Update Service, Automatic subsequent deliveries of Upgrades and service packs for one year with automatic extension; requires current software version; only valid in connection with Unlock Copy License agreement; Minimum ordering quantity 20 units ******************************* E-mail address required for delivery",116,"ST",1,"SIMATIC",1E-3,1,"6AV66120AA000UY0"]
["6AV6612-0AA01-0AQ0","EPL Royalty for WinCC flexible Standard, only valid in connection with Enterprise License agreement, requires EPL Master",1601,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV66120AA010AQ0"]
["6AV6612-0AA01-3UC0","WinCC flexible 2008 Standard UCL package for one installation; Engineering SW; SW and documentation on DVD; Master license on CD-ROM; UCL agreement required",961,"ST",1,"SIMATIC",0.23599999999999999,1,"6AV66120AA013UC0"]
["6AV6612-0AA01-3UE3","WinCC flexible 2008 Standard Unlock Copy License (UCL), MLK update for 64-bit operating systems only valid in connection with Unlock Copy License agreement",39.700000000000003,"ST",1,"SIMATIC",0.17399999999999999,1,"6AV66120AA013UE3"]
["6AV6612-0AA01-3UF0","WinCC flexible 2008 Standard Upgrade incl. Change Control, Unlock Copy License (UCL), Expansion package for 5 installations, only valid in connection with Unlock Copy License agreement",1211,"ST",1,"SIMATIC",5.2999999999999999E-2,1,"6AV66120AA013UF0"]
["6AV6612-0AA01-3UH0","WinCC flexible 2008 Standard UCL Package for one installation; engineering software; software, documentation and master license for download; only valid with UCL agreement ******************************* email address is mandatory for delivery",867,"ST",1,"SIMATIC",1E-3,1,"6AV66120AA013UH0"]
["6AV6612-0AA11-3CE5","WinCC flexible 2008 Asia standard, Upgrade for WinCC flexible 2004/2005/2007 Asia Standard, incl. Change Control, Engineering software,Floating license License key on USB stick, SW and documentation on DVD, en/chs/cht/kor/jap, executable under XP Prof/ Windows7 Professional/Ultimate/ Enterprise (32/64 bit)",430,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV66120AA113CE5"]
["6AV6612-0AA31-3CA8","WinCC flexible 2008 China standard, Engineering software, Single license, SW and documentation on DVD in Chinese Simplified, executable under XP Prof/ Windows7 Professional/Ultimate/ Enterprise (32/64 bit), for configuration of SIMATIC Panels",134,"ST",1,"SIMATIC",0.185,1,"6AV66120AA313CA8"]
["6AV6612-0AA51-3CA5","WinCC flexible 2008 Standard engineering software,Floating License license key on USB flash drive, SW and documentation on DVD in de/en/fr/it/sp/zh-s/zh-t/kor/ja p executable in Windows 7 Prof/Ultimate/Enterprise(32/64) Windows 10 Pro/Enterprise (64), for configuration of SIMATIC Panels ******************************* Content: Set (1x DVD + 1x USB)",1696,"ST",1,"SIMATIC",0.21099999999999999,1,"6AV66120AA513CA5"]
["6AV6612-0AA51-3CE5","WinCC flexible 2008 Standard, upgrade for WinCC flexible 2004/2005/2007 Standard, incl. Change Control, engineering software,Floating License license key on USB flash drive, SW and documentation on DVD, de/en/fr/it/sp/zh-s/zh-t/kor/ja p, executable in Windows 7 Prof/Ultimate/Enterprise(32/64) Windows 10 Pro/Enterprise (64) ******************************* Content: Set (1x DVD + 1x USB)",430,"ST",1,"SIMATIC",0.21099999999999999,1,"6AV66120AA513CE5"]
["6AV6612-0AA51-3CH5","WinCC flexible 2008 Standard Engineering software,Floating License Software and License key download, d/e/f/i/s/chs/cht/kor/jap Executable under Windows 7 Prof/Ultimate/Enterprise(32/64) Windows 10 Prof/Enterprise (64), for configuration of SIMATIC Panels ******************************* E-mail address required for delivery",1453,"ST",1,"SIMATIC",1E-3,1,"6AV66120AA513CH5"]
["6AV6612-0AA51-3CK5","WinCC flexible 2008 Standard, Upgrade for WinCC flexible 2004/2005/2007 Standard, incl. Change Control, Engineering SW,Floating License Software and License key download, d/e/f/i/s/chs/cht/kor/jap, Executable under Windows 7 Prof/Ultimate/Enterprise(32/64) Windows 10 Prof/Enterprise (64) ******************************* E-mail address required for delivery",368,"ST",1,"SIMATIC",1E-3,1,"6AV66120AA513CK5"]
["6AV6612-2BC01-3AD5","WinCC flexible 2008 Standard Powerpack for WinCC flexible 2008 Compact Engineering software, floating license, license key on USB flash drive ******************************* Content: 1x USB",1354,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV66122BC013AD5"]
["6AV6612-2BC01-3AJ5","WinCC flexible 2008 Standard Power Pack for WinCC flexible 2008 Compact, Engineering software, floating license License key download ******************************* E-mail address required for delivery",1160,"ST",1,"SIMATIC",1E-3,1,"6AV66122BC013AJ5"]
["6AV6612-8AA00-0AR0","EPL-Maintenance WinCC flexible standard (EPL=Enterprise License) Payment for maintenance of a Royalty for 12 months, only valid in connection with Enterprise License contract, requires EPL Master",245,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV66128AA000AR0"]
["6AV6613-0AA00-0AL0","SIMATIC WinCC Advanced Software Update Service within the framework of this contract, you will receive for one year all up-to-date software versions. the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software",387,"ST",1,"SIMATIC",0.2,1,"6AV66130AA000AL0"]
["6AV6613-0AA00-0AM0","SIMATIC WinCC Advanced Software Update Service Compact for multiple orders on one position, these deliveries are grouped. Minimum order quantity: 3 units within the framework of this contract, you will receive for one year all up-to-date software versions. the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software",387,"ST",1,"SIMATIC",1.2E-2,1,"6AV66130AA000AM0"]
["6AV6613-0AA00-0AY0","SIMATIC WinCC Advanced SUS (download) Software Update Service, within the framework of this contract, you will receive for one year all up-to-date software versions, the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software ******************************* E-mail address required for delivery",361,"ST",1,"SIMATIC",1E-3,1,"6AV66130AA000AY0"]
["6AV6613-0AA00-0UL0","SIMATIC WinCC Advanced Unlock Copy License (UCL) Software Update Service, Automatic subsequent deliveries of upgrades and service packs for one year with automatic extension, requires current software version, only valid in connection with Unlock Copy License agreement Minimum ordering quantity 20 units",227,"ST",1,"SIMATIC",1.2E-2,1,"6AV66130AA000UL0"]
["6AV6613-0AA00-0UY0","SIMATIC WinCC Advanced SUS (UCL download) Software Update Service, Automatic subsequent deliveries of Upgrades and service packs for one year with automatic extension; requires current software version; only valid in connection with Unlock Copy License agreement; Minimum ordering quantity 20 units ******************************* E-mail address required for delivery",216,"ST",1,"SIMATIC",1E-3,1,"6AV66130AA000UY0"]
["6AV6613-0AA01-0AQ0","EPL Royalty for WinCC flexible Advanced, only valid in connection with Enterprise License agreement, requires EPL Master",2829,"ST",1,"SIMATIC",1.0999999999999999E-2,1,"6AV66130AA010AQ0"]
["6AV6613-0AA01-3UC0","WinCC flexible 2008 Advanced UCL package for one installation; Engineering SW; SW and documentation on DVD; Master license on CD-ROM; UCL agreement required",1699,"ST",1,"SIMATIC",0.23599999999999999,1,"6AV66130AA013UC0"]
["6AV6613-0AA01-3UE3","WinCC flexible 2008 Advanced Unlock Copy License (UCL), MLK update for 64-bit operating systems only valid in connection with Unlock Copy License agreement",39.700000000000003,"ST",1,"SIMATIC",0.17399999999999999,1,"6AV66130AA013UE3"]
["6AV6613-0AA01-3UF0","WinCC flexible 2008 Advanced Upgrade incl. Change Control, Unlock Copy License (UCL), Expansion package for 5 installations, only valid in connection with Unlock Copy License agreement",2183,"ST",1,"SIMATIC",5.2999999999999999E-2,1,"6AV66130AA013UF0"]
["6AV6613-0AA01-3UH0","WinCC flexible 2008 Advanced UCL package for one installation; Engineering software; Software, documentation and master license for download; UCL agreement required ******************************* E-mail address required for delivery",1533,"ST",1,"SIMATIC",1E-3,1,"6AV66130AA013UH0"]
["6AV6613-0AA11-3CE5","WinCC flexible 2008 Asia Advanced, Upgrade for WinCC flexible 2004/2005/2007 Asia Advanced, incl. Change Control, Engineering software,Floating license License key on USB stick, SW and documentation on DVD, en/chs/cht/kor/jap, executable under XP Prof/ Windows7 Professional/Ultimate/ Enterprise (32/64 bit)",754,"ST",1,"SIMATIC",0.20300000000000001,1,"6AV66130AA113CE5"]
["6AV6613-0AA51-3CA5","WinCC flexible 2008 Advanced engineering software,Floating License license key on USB flash drive, SW and documentation on DVD in de/en/fr/it/sp/zh-s/zh-t/kor/ja p executable in Windows 7 Prof/Ultimate/Enterprise(32/64) Windows 10 Pro/Enterprise (64), for configuration of SIMATIC Panels and WinCC flexible 2008 Runtime ******************************* Content: Set (1x DVD + 1x USB)",2999,"ST",1,"SIMATIC",0.21099999999999999,1,"6AV66130AA513CA5"]
["6AV6613-2BD01-3AJ5","WinCC flexible 2008 Advanced Power Pack for WinCC flexible 2008 Compact engineering software, floating license License key download ******************************* E-mail address required for delivery",2275,"ST",1,"SIMATIC",1E-3,1,"6AV66132BD013AJ5"]
["6AV6671-8XJ00-0AX0","Converter RS422 to TTY Converter RS422 to TTY, female (15-pin), can be screwed together with RS422 interface, Cable outlet 180 degrees, for connection of SIMATIC S5",121,"ST",1,"SIMATIC",5.1999999999999998E-2,1,"6AV66718XJ000AX0"]
["6AV7230-0CA20-1BA0","SIMATIC IPC377E (BASICPANEL PC) 12\" TOUCH; CELERON N3160 (4C/4T); 4 GB RAM; 500 GB HDD; 1x DISPLAY-PORT GRAPHIC; 1x VGA-PORT GRAPHIC; 2x 10/100/1000 MBIT/S ETHERNET RJ45; 2x USB3.0, 2x USB2.0; 4x COM-PORTS; 1x mPCIe-SLOT; 1x mSATA-SLOT; WINDOWS 7 ULT. 64 BIT 24V DC POWER SUPPLY; PANEL MOUNT",2457,"ST",1,"SIMATIC",3.6,1,"6AV72300CA201BA0"]
["6AV7466-6MA02-0CS0","SIMATIC IFP1900 PRO HD LR Flat Panel 19\" display (16:9), Multitouch, Full HD resolution, Prepared for support arm/pedestal and expansion elements; Extended version up to 30 m, 1920 x 1080 pixels, for 24 V DC, display port/DVI interface IP65 fully enclosed with adaptation for extensions left and right with flange mount with basic adapter mounting material",2347,"ST",1,"SIMATIC",9.1999999999999993,1,"6AV74666MA020CS0"]
["6AV7675-0NR00-0AA0","Transport in wooden box for Panel PC Ex and Thin Client Ex without enclosure",212,"ST",1,"SIMATIC",10,1,"6AV76750NR000AA0"]
["6AV9681-1AA12-0AX0","WinCC/SYSTEMDIAGNOSTIC V7.0 PROFINET IO Device Diagnostic Diagnostics of slaves with detailed information released for WinCC V6.0.2-V7.0",520,"ST",1,"SIMATIC",0.20100000000000001,1,"6AV96811AA120AX0"]
["6BK1942-6KA00-0AA0","Replacement part SIPLUS HCS4200 Fuse for POM4220 Highend 25A/600V",258,"PAK",1,"SIMATIC",1E-3,1,"6BK19426KA000AA0"]
["6DD1660-0BH1","SIMATIC TDC COMMUNICATION MODULE CP52A0 ACCESS MODULE FOR GLOBAL DATA MEMORY (GDM)",5869,"ST",1,"SIMATIC",0.46800000000000003,1,"6DD16600BH1"]
["6EP1935-6MC01","SITOP rechargeable battery module 24 V/1.2 Ah with maintenance free Seaed lead batteries for SITOP DC-USV Module 6 A",98.7,"ST",1,"SIMATIC",1.65,1,"6EP19356MC01"]
["6EP3321-6SB00-0AY0","LOGO!POWER 12 V / 1.9 A Stabilized power supply input: 100-240 V AC output: 12 V DC/ 1.9 A",72.5,"ST",1,"SIMATIC",0.14000000000000001,1,"6EP33216SB000AY0"]
["6ES5497-4UC11","SIMATIC, Release tool for crimp contacts",15,"ST",1,"SIMATIC",0.2,1,"6ES54974UC11"]
["6ES7134-6HD01-0BA1","SIMATIC ET 200SP, ANALOG INPUT MODULE, AI 4XU/I 2-WIRE STANDARD, PACKING UNIT: 1 PIECE, FITS TO BU-TYPE A0, A1, COLOR CODE CC03, MODULE DIAGNOSIS, 16BIT, +/-0,3%",164,"ST",1,"SIMATIC",4.1000000000000002E-2,1,"6ES71346HD010BA1"]
["6ES7148-6JA00-0AB0","SIMATIC DP, ET 200ECO PN, IO-Link master, 4IO-L+8DI+4DO 24 V DC/1.3A 8xM12, Duplicate assignment, Degree of protection IP67",492,"ST",1,"SIMATIC",0.97099999999999997,1,"6ES71486JA000AB0"]
["6ES7155-6AU00-0AB2","training pack SIMATIC ET 200SP IO-Link Consisting of: 1x IM155-6PN HF, 1x BusAdapter BA 2xRJ45, 2x DI 8x 24 V DC/0.5 A HF, 2x DQ 8x 24 V DC/0.5 A HF, 1x CM 4XIO-Link, 5x BASE UNITS, Labeling strips, color identification labels ******************************* for educational purposes only",894,"ST",1,"SIMATIC",1.4,1,"6ES71556AU000AB2"]
["6ES7193-6LF30-0AW0","SIMATIC ET 200SP, 160 reference designation labels, 10 mats (160 labels), for BA, BU, IM and I/O modules",26.8,"PAK",1,"SIMATIC",0.123,1,"6ES71936LF300AW0"]
["6ES7194-2MH02-1AA0","Power cable M8, PUR cable both ends assembled with M8 connector and M8 socket, 4-pole, length 0.19 m",14.5,"ST",1,"SIMATIC",2.1999999999999999E-2,1,"6ES71942MH021AA0"]
["6ES7194-2MN15-1AA0","Power cable M8, PUR cable both ends assembled with M8 connector and M8 socket, 4-pole, Length 15 m",57.1,"ST",1,"SIMATIC",0.58899999999999997,1,"6ES71942MN151AA0"]
["6ES7215-1HG40-4AB8","training pack CPU 1215C DC/DC/RLY, Consisting of: 6x S7-1200 CPU 1215C DC/DC/RLY, 6x STEP 7 Basic Single License, 6x SIMATIC Memory Card 4 MB 6x RJ45 cable, Length 6m, ******************************* for educational purposes only",2085,"ST",1,"SIMATIC",5.7,1,"6ES72151HG404AB8"]
["6ES7317-7TK10-0AB0","SIMATIC S7-300, CPU 317T-3 PN/DP, Central processing unit for PLC and technology tasks, 1024 KB work memory, 1st interface MPI/DP 12 Mbit/s, 2nd interface DP (drive), 3rd interface Ethernet PROFINET with 2-port switch, Integr. I/O for technology, Front connector (1x 40-pole) and Micro Memory Card min. 8 MB required",5432,"ST",1,"SIMATIC",0.73599999999999999,1,"6ES73177TK100AB0"]
["6ES7332-5HF00-0AB0","SIMATIC S7-300, Analog output SM 332, isolated, 8 AO, U/I; diagnostics; resolution 11/12 bits, 40-pole, removing and inserting possible with active backplane bus",1140,"ST",1,"SIMATIC",0.32600000000000001,1,"6ES73325HF000AB0"]
["6ES7414-2XL07-0AB0","SIMATIC S7-400, CPU 414-2 Central processing unit with: Work memory 2 MB, (1 MB code, 1 MB data), 1st interface MPI/DP 12 Mbit/s, 2nd interface PROFIBUS DP,",3945,"ST",1,"SIMATIC",0.89800000000000002,1,"6ES74142XL070AB0"]
["6ES7490-1BA00-0AA0","SIMATIC S7/M7, connection terminal for modules 6 units per packing unit",17.900000000000002,"PAK",1,"SIMATIC",5.7000000000000002E-2,1,"6ES74901BA000AA0"]
["6ES7511-1FK02-0AB0","SIMATIC S7-1500F, CPU 1511F-1 PN, CENTRAL PROCESSING UNIT WITH WITH WORKING MEMORY 225 KB FOR PROGRAM AND 1 MB FOR DATA, 1. INTERFACE: PROFINET IRT WITH 2 PORT SWITCH, 60 NS BIT-PERFORMANCE, SIMATIC MEMORY CARD NECESSARY",943,"ST",1,"SIMATIC",0.439,1,"6ES75111FK020AB0"]
["6ES7592-2AX00-0AA0","SIMATIC S7-1500, Labeling sheets for 35 mm wide S7-1500 modules Color: AL GREY Material: foil, perforated; suitable for printing using commercially available laser printers; 10 sheets with 10 strips each per packing unit sufficient for 100 modules",52.5,"PAK",1,"SIMATIC",0.224,1,"6ES75922AX000AA0"]
["6ES7648-2BF08-0XC0","SIMATIC PC, CompactFlash, 256 MByte, Industrial Grade",73.5,"ST",1,"SIMATIC",3.2000000000000001E-2,1,"6ES76482BF080XC0"]
["6ES7810-4CC11-2YE0","SIMATIC S7, STEP 7 V5.6 SP1, Unlock Copy License (UCL), UCL upgrade (V5.5 to V5.6) for 1 installation, only valid in connection with Unlock Copy License agreement requires UCL basic package Minimum ordering quantity 20 units ******************************* Content: set (1x DVD + 1x CD)",323,"ST",1,"SIMATIC",0.22600000000000001,1,"6ES78104CC112YE0"]
["6ES7823-0AA00-1DA0","SIMATIC ProDiag S7-1500, Single Runtime License, contains license certificate for activation of all configured monitoring processes in a CPU, Class A, executable on all S7-1500 Firmware V2.0 or higher ******************************* Content: Certificate of License",707,"ST",1,"SIMATIC",2.8000000000000001E-2,1,"6ES78230AA001DA0"]
["6ES7833-1FC02-0YE5","SIMATIC S7, F-programming tool S7 Distributed Safety V5.4, upgrade from V5.X to V5.4, floating license for 1 user, E-SW, SW and documentation on DVD, Class A, 3 languages (de,en,fr), executable in Windows 7 SP1, Windows 10 Professional, Windows 10 Enterprise, Windows Server 2008 R2 SP1, Windows Server 2012 R2, Windows Server 2016; 64-bit operating system required; STEP 7 V5.5 SP1 or higher; Ref,-HW S7-300F/400F/WinAC F",293,"ST",1,"SIMATIC",0.21199999999999999,1,"6ES78331FC020YE5"]
["6ES7853-0AA01-0YE5","Siemens Network Planner Upgrade V2.0, Floating License; Software for simulation of PROFINET networks; Software and documentation on DVD; license key on a USB flash drive; Class A; 3 languages: de, en, zh; executable on Windows 7 (64 bit) and Windows 10 (64 bit)",389,"ST",1,"SIMATIC",0.20100000000000001,1,"6ES78530AA010YE5"]
["6ES7922-4BD20-5AD0","Front connector for SIMATIC S7-400 48-pol strip for MS/MSP/MR units (6ES7492-1AL00-0AA0) with 46 single cores 0.5 mm2, Single cores H05V-K, Screw version VPE=5 units L = 3.2 m",537,"PAK",1,"SIMATIC",7.55,1,"6ES79224BD205AD0"]
["6ES7922-5CB00-0AB0","Front connector for SIMATIC S7-1500 40 pole (6ES7592-1AM00-0XB0) with 20 single cores 0.5 mm2 (1-20) Core type H05V-K Screw version L = 10.0 m",116,"ST",1,"SIMATIC",2.14,1,"6ES79225CB000AB0"]
["6ES7923-5BJ00-0EB0","Connecting cable unshielded f. SIMATIC S7-300/1500 0.14 mm2 between front connector module 4 x 16 pole and connection module 1 x 50 pole with IDC connectors, L = 8.0 m",103,"ST",1,"SIMATIC",1.498,1,"6ES79235BJ000EB0"]
["6ES7972-0DA00-0AA0","SIMATIC DP, RS485 terminating resistor for terminating PROFIBUS/MPI networks",87,"ST",1,"SIMATIC",0.105,1,"6ES79720DA000AA0"]
["6FB1231-3BM12-7AT0","SIDOOR ATE530S COATED Control device for Platform doors, with protective coating, up to 280 kg door weight, 1*RS485, 5*DI, 2*DO, -25-+50 Β°C PROFINET IO Conformance Class C via 2x RJ45 sockets",1386,"ST",1,"SIMATIC",0.95699999999999996,1,"6FB12313BM127AT0"]
["6GF3440-8CD01","MV440-MV500 ring light holder for SIMATIC VS100 ring lamps; suitable for 6GF9004-7AA01, ... - 7BA01,...- 8BA01,...- 8C0, ...- 8DA1 and 6GF3400-0LT0-7BA1 and 6GF3400-0LT0-8DA1 screws enclosed WxHxD (mm) 175x 225x 3",91.699999999999989,"ST",1,"SIMATIC",0.2,1,"6GF34408CD01"]
["6GK1500-0AA10","Bus terminal 12M for PROFIBUS, Transmission rates 9.6 Kbit/s to 12 Mbit/s, Plug-in cable 1.5 m",158,"ST",1,"SIMATIC",0.35099999999999998,1,"6GK15000AA10"]
["6GK1706-1CW13-0AA0","Industrial Ethernet S7 OPC Redundancy V13 for CP 1612 A2, CP 1613 A2, CP 1623, CP 1628 redundant OPC Server software Pair for IE software S7 products Single License for 2 installations; Runtime software, Software and electr. manual on DVD; License key on USB stick; Class A; 2 languages (de, en); for Windows Server 2008 R2 SP1",1470,"ST",1,"SIMATIC",0.30099999999999999,1,"6GK17061CW130AA0"]
["6GK1716-0HB14-0AK1","POWERPACK HARDNET IE S7-REDCONNECT V14; Expansion HARDNET-IE S7 V14; to HARDNET-IE S7-REDCONNECT; Floating License R-SW, SW + electr. manual; License key for download; Class A; 2 languages (d,e); for 32/64 Bit: Win 7 SP1 Prof/Ult, 64Bit: Win 8.1 PRO; Windows 10, Server 2008 R2 SP1, 2012 R2 max. 4 CP1613A2, CP1623, CP1628 ******************************* E-mail address required for delivery",1040,"ST",1,"SIMATIC",1E-3,1,"6GK17160HB140AK1"]
["6GK1901-1BK00-0AA2","Industrial Ethernet Insert 1GE for modular outlet base module, Interchangeable insert with 1 x 1000 Mbit RJ45 interface 1 pack=4 units",80.3,"PAK",1,"SIMATIC",0.3,1,"6GK19011BK000AA2"]
["6GK1905-6PB00","PROFIBUS Plastic Fiber Optic, BFOC crimping tool",378,"ST",1,"SIMATIC",0.66,1,"6GK19056PB00"]
["6GK5308-2GG10-2CA2","SCALANCE X308-2M TS;  managed IE switch, compact; 4x 10/100/1000 Mbit/s for RJ45 ports electrical; 2x 100/1000 Mbit/s for 2-port media modules, electrical or optical; LED diagnostics; error signaling Contact; PROFINET IO device; network management; integrated redundancy manager; Office features (RSTP, VLAN, IGMP,..); C-plug in scope of delivery extended temperature range with railway approval EN 50155;",2457,"ST",1,"SIMATIC",1,1,"6GK53082GG102CA2"]
["6GK5400-8AS00-8AP2","PE400-8SFP Port Extender for SCALANCE XM-400 managed modular IE switch; extension by 8x 100/1000 Mbit/s SFP",1365,"ST",1,"SIMATIC",0.77200000000000002,1,"6GK54008AS008AP2"]
["6GK5795-6MP00-0AA0","ANT795-6MP IWLAN antenna with omnidirectional characteristic incl. N-female connector: 5/7 dBi; IP65/67 (-40 - +80 Β°C); 2.4/5 GHz Wi-Fi compliance and national approvals to be observed; Mounting on wall or mast; compact instructions in German/English Scope of delivery: 1x ANT795-6MP, 1 x mounting aid",221,"ST",1,"SIMATIC",0.14000000000000001,1,"6GK57956MP000AA0"]
["6GK5907-8UA00-0AA0","SCALANCE CLP 2GB W1780 iFeatures Removable data storage medium for enabling iFeatures for SCALANCE W in Access Point Mode permits simple device replacement in case of fault, and the recording of configuration data, or configuration and application data, for all SCALANCE W1700 devices",420,"ST",1,"SIMATIC",3.0000000000000001E-3,1,"6GK59078UA000AA0"]
["6GK7542-6VX00-0XE0","Communications Processor CP 1542SP-1 IRC for connection of an SIMATIC S7-ET 200SP to Industrial Ethernet, SINAUT ST7, TeleControl Server Basic, IEC-60870-5-104 or DNP3 protocol to a control center; Open IE communication (TCP/IP, ISO-on-TCP, UDP), IP broadcast/multicast, SNMPV1, DHCP, Secure e-Mail, IPV4/IPV6, support of SINEMA Remote Connect with autoconfiguration; time-of-day synchronization via NTP, access to web server of the CPU, bus adapter required",783,"ST",1,"SIMATIC",0.20100000000000001,1,"6GK75426VX000XE0"]
["6GT2300-0AA00","MOBY E mobile data memory MDS E600 ISO card, 752 bytes EEPROM, IP68, -25 ... +60 Β°C, 85x 54x 0.8 mm",19.8,"ST",1,"SIMATIC",5.0000000000000001E-3,1,"6GT23000AA00"]
["6GT2780-0DC20","SIMATIC RTLS Locating Manager Initial position detection 1000 for 1,000 transponders, option for license Basic, Single License, software and license key download ******************************* E-mail address required for delivery",11550,"ST",1,"SIMATIC",1E-3,1,"6GT27800DC20"]
["6GT2810-2AB03","SIMATIC RF630L SmartLabel Inlay PET; 54x 34 mm; ISO 18000-6C, EPC Class 1 GEN 2 frequency 860 to 960 MHz, Chip Type NXP G2XM 240-bit EPC memory, 64 bytes Add-on memory 2000 units on one roll Minimum order quantity 2000 units",55.5,"ST",100,"SIMATIC",0.01,1,"6GT28102AB03"]
["6GT2891-4FN50","SIMATIC RF, MV plug-in cable, assembled, between ASM 456, RF160C, RF170C, RF18XC and reader, or extension cable for ASM 456, RF160C, RF170C, RF18XC with RF, MV, MOBY PUR, trailing, length 50 m",235,"ST",1,"SIMATIC",2.9049999999999998,1,"6GT28914FN50"]
["6NH3112-3BA00-1XX3","Degree of protection of aluminum enclosure IP68; suitable for SIMATIC RTU3000C; temperature range -40 to +80 Β°C; Cover with pin-torx screws; 7 Cable bushings and bushing for mobile radio antenna prepared; Please Cable glands and sealing plugs in the required number separately order",294,"ST",1,"SIMATIC",3.395,1,"6NH31123BA001XX3"]
["6NH9910-0AA31-0AF0","TeleControl Server Basic 32 V3.1; Single License for 1 installation; OPC (UA) - Server for IP communication with S7-1200, ET200SP, RTU3000C; Connection management of 32 RTUs; Routing between RTUs; multiproject-capable; Connection diagnose; Station monitoring; German and English User interface",1743,"ST",1,"SIMATIC",0.19800000000000001,1,"6NH99100AA310AF0"]
["6XV1821-0BN30","PROFIBUS Plastic Fiber Optic, Standard cable with 4 BFOC connectors, Length 30 m",167,"ST",1,"SIMATIC",1.9,1,"6XV18210BN30"]
["6XV1850-2HH20","Industrial Ethernet TP XP Cord RJ45/RJ45, TP cord Pre-assembled with 2 RJ45 connector, Send and receive line crossed, Length 2 m",14,"ST",1,"SIMATIC",0.08,1,"6XV18502HH20"]
["6XV1870-3QE50","Industrial Ethernet TP Cord RJ45/RJ45, CAT 6A, TP cable 4x2, pre-assembled with 2 RJ45 connectors, Length 0.5 m",17.5,"ST",1,"SIMATIC",3.6999999999999998E-2,1,"6XV18703QE50"]
["6XV1870-8GH20","IE Connecting Cable M12-90/M12-90, pre-assembled IE FC Trailing Cable GP, with 2 M12 connectors (D-coded) Length 2.0 m",30.5,"ST",1,"SIMATIC",0.18,1,"6XV18708GH20"]
["6XV1875-5CH20","N-Connect/ R-SMA male/male flexible connection cable pre-assembled, length 2 m flexible connecting cable Access point antenna (RCoax and others)",43.4,"ST",1,"SIMATIC",0.2,1,"6XV18755CH20"]
["6XV1878-5BN30","IE connecting cable IE FC RJ45 Plug-180/IE FC RJ45 Plug-180; IE FC flexible GP 4x2 cable Pre-assembled with 2x IE FC RJ45 plug 180 4 x 2; Length 30 m",147,"ST",1,"SIMATIC",2.56,1,"6XV18785BN30"]
["7KG6106-2QN27-0B","Simeas transmitter (G) MUU for alternating voltage in the enclosure, for snapping on standard mounting rail Rated frequency 50 Hz Input voltage 250 V AC Output signal DC 4 to 20 mA (live zero) Auxiliary power 45 to 65 Hz AC, 230 V Measuring range linear 0 up to UEN",645,"ST",1,"SIMATIC",0.33,1,"7KG61062QN270B"]
["7KG6113-2EN27-0B","Simeas transmitter (G) MUI for alternating current in the enclosure, for snapping on standard mounting rail Rated frequency 50 Hz Input current 5 A Output signal DC 4 to 20 mA (live zero) Auxiliary power 45-65 Hz AC, 230 V Measuring range linear 0 up to IEN",645,"ST",1,"SIMATIC",0.33,1,"7KG61132EN270B"]
["A5E36805208","SIMATIC S7-1500F, CPU 1516F-3 PN/DP, Central processing unit with work memory 1.5 MB for program and 5 MB for data, 1st interface: PROFINET IRT with 2-port switch, 2nd interface: PROFINET RT, 3rd interface: PROFIBUS, 10 ns bit performance, SIMATIC Memory Card required, without display",4190,"ST",1,"SIMATIC",0.90100000000000002,1,"A5E36805208"]
["EWK:10660305","SCALANCE S SRS enabled bundle consisting of SCALANCE S613 and Healthcare CRSP Install. WIZARD CD-ROM",1953,"ST",1,"SIMATIC",1,1,"EWK:10660305"]
["1FK2203-2AG00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm; Converter at max. 240 V supply system; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; Connector size M12, rotatable;",1225,"ST",1,"MC",2.29,1,"1FK22032AG000MA0"]
["1FK2203-4AG10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm; Converter at max. 240 V supply system; With holding brake; Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22 bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1292,"ST",1,"MC",3.29,1,"1FK22034AG101SA0"]
["1FK7015-5AK24-1JG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1303,"ST",1,"MC",1.1020000000000001,1,"1FK70155AK241JG3"]
["1FK7022-5AK21-1DB5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2419,"ST",1,"MC",2.0019999999999998,1,"1FK70225AK211DB5"]
["1FK7022-5AK21-1SH8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR Resolver multi-pole (resolver P=3) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1501,"ST",1,"MC",2.0019999999999998,1,"1FK70225AK211SH8"]
["1FK7022-5AK21-1VG8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2022,"ST",1,"MC",1.8029999999999999,1,"1FK70225AK211VG8"]
["1FK7022-5AK71-1PA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1463,"ST",1,"MC",1.8029999999999999,1,"1FK70225AK711PA2"]
["1FK7022-5AK71-1SB8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR Resolver multi-pole (resolver P=3) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1601,"ST",1,"MC",2.0019999999999998,1,"1FK70225AK711SB8"]
["1FK7022-5AK71-1VG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1753,"ST",1,"MC",1.8029999999999999,1,"1FK70225AK711VG0"]
["1FK7024-5AK71-8JG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, 1.1Nm 100K, 6000rpm, 0.50kW Naturally cooled IM B5 (IM V1, IM V3) Bare cable end 0.5m Outlet directions DE with connector size 1 absolute encoder 16 S/R (encoder A-16); Derating 10% due to Absolute encoder; smooth shaft, Tolerance N without holding brake; Degree of protection IP64",1924,"ST",1,"MC",2,1,"1FK70245AK718JG0"]
["1FK7032-2AF21-1FB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2681,"ST",1,"MC",3,1,"1FK70322AF211FB0"]
["1FK7032-2AK71-1CH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2500,"ST",1,"MC",3,1,"1FK70322AK711CH0"]
["1FK7032-2AK71-1TH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1318,"ST",1,"MC",3.0009999999999999,1,"1FK70322AK711TH2"]
["1FK7032-5AF21-1AH3","SIMOTICS S Synchronous servo motor 1FK7 Compact DC link 300V 1.1Nm, 100K, 3000 rpm 0.31kW, Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2308,"ST",1,"MC",3.0019999999999998,1,"1FK70325AF211AH3"]
["1FK7032-5AF21-1HG0","SIMOTICS S Synchronous servo motor 1FK7 Compact DC link 300V 1.1Nm, 100K, 3000 rpm 0.31kW, Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2451,"ST",1,"MC",2.7029999999999998,1,"1FK70325AF211HG0"]
["1FK7032-5AF21-1VA5","SIMOTICS S Synchronous servo motor 1FK7 Compact DC link 300V 1.1Nm, 100K, 3000 rpm 0.31kW, Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2382,"ST",1,"MC",2.7029999999999998,1,"1FK70325AF211VA5"]
["1FK7032-5AK71-1AH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 1.1Nm, 100K, 6000rpm 0.50kW, Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2371,"ST",1,"MC",3.0019999999999998,1,"1FK70325AK711AH2"]
["1FK7032-5AK71-1LB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 1.1Nm, 100K, 6000rpm 0.50kW, Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3221,"ST",1,"MC",3.0019999999999998,1,"1FK70325AK711LB3"]
["1FK7032-5AK71-1VA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 1.1Nm, 100K, 6000rpm 0.50kW, Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2382,"ST",1,"MC",2.7029999999999998,1,"1FK70325AK711VA5"]
["1FK7033-4CF21-1SA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1226,"ST",1,"MC",3.0019999999999998,1,"1FK70334CF211SA1"]
["1FK7033-4CF21-1UH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1624,"ST",1,"MC",3.3010000000000002,1,"1FK70334CF211UH1"]
["1FK7033-4CK74-1AG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1662,"ST",1,"MC",3.0009999999999999,1,"1FK70334CK741AG0"]
["1FK7033-4CK74-1TB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1361,"ST",1,"MC",3.3010000000000002,1,"1FK70334CK741TB0"]
["1FK7033-7AF21-1JA8","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic, DC link 300V 1, 3 Nm, 100K, 3000 rpm Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2257,"ST",1,"MC",3.1030000000000002,1,"1FK70337AF211JA8"]
["1FK7033-7AF21-1TH5","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic, DC link 300V 1, 3 Nm, 100K, 3000 rpm Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1723,"ST",1,"MC",3.4020000000000001,1,"1FK70337AF211TH5"]
["1FK7033-7AK71-1JB8","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic 1, 3 Nm, 100K, 6000rpm 0.57kW, Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2543,"ST",1,"MC",3.4020000000000001,1,"1FK70337AK711JB8"]
["1FK7033-7AK71-1SA8","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic 1, 3 Nm, 100K, 6000rpm 0.57kW, Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1684,"ST",1,"MC",3.1030000000000002,1,"1FK70337AK711SA8"]
["1FK7033-7AK71-1TH3","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic 1, 3 Nm, 100K, 6000rpm 0.57kW, Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1601,"ST",1,"MC",3.4020000000000001,1,"1FK70337AK711TH3"]
["1FK7034-2AF21-1DG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2060,"ST",1,"MC",3.702,1,"1FK70342AF211DG0"]
["1FK7034-2AF21-1UA2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1539,"ST",1,"MC",3.702,1,"1FK70342AF211UA2"]
["1FK7034-2AK71-1RH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 20 bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQI) smooth shaft, Tolerance N with holding brake Degree of protection IP65 DE flange IP67",2190,"ST",1,"MC",4,1,"1FK70342AK711RH2"]
["1FK7034-2AK74-1EG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2114,"ST",1,"MC",3.7010000000000001,1,"1FK70342AK741EG0"]
["1FK7034-5AF21-1LA2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 1.6Nm, 100K, 3000 rpm 0.46kW, Naturally cooled power/signal connectors Connector can be rotated by 270Β° ABSOLUTE ENCODER 512 S/R (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3122,"ST",1,"MC",3.7029999999999998,1,"1FK70345AF211LA2"]
["1FK7034-5AF21-1TB5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 1.6Nm, 100K, 3000 rpm 0.46kW, Naturally cooled power/signal connectors Connector can be rotated by 270Β° RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1905,"ST",1,"MC",4.0019999999999998,1,"1FK70345AF211TB5"]
["1FK7034-5AK71-1HB5","SIMOTICS S Synchronous servo motor 1FK7 Compact, 1.6Nm 100K, 6000rpm, 0.63kW Naturally cooled power/signal connectors Connector can be rotated by 270Β° ABSOLUTE ENCODER 512 S/R (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3155,"ST",1,"MC",4.0019999999999998,1,"1FK70345AK711HB5"]
["1FK7034-5AK71-1LA2","SIMOTICS S Synchronous servo motor 1FK7 Compact, 1.6Nm 100K, 6000rpm, 0.63kW Naturally cooled power/signal connectors Connector can be rotated by 270Β° ABSOLUTE ENCODER 512 S/R (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3122,"ST",1,"MC",3.7029999999999998,1,"1FK70345AK711LA2"]
["1FK7034-5AK71-1SH2","SIMOTICS S Synchronous servo motor 1FK7 Compact, 1.6Nm 100K, 6000rpm, 0.63kW Naturally cooled power/signal connectors Connector can be rotated by 270Β° RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1730,"ST",1,"MC",4.0019999999999998,1,"1FK70345AK711SH2"]
["1FK7040-2AK71-1EB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.69kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2453,"ST",1,"MC",3.5,1,"1FK70402AK711EB0"]
["1FK7040-2AK71-1RH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.69kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2202,"ST",1,"MC",3.5,1,"1FK70402AK711RH2"]
["1FK7040-5AK71-1DG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 1.6Nm, 100K, 6000rpm 0.69kW, Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2546,"ST",1,"MC",3.5030000000000001,1,"1FK70405AK711DG5"]
["1FK7040-5AK71-1FB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 1.6Nm, 100K, 6000rpm 0.69kW, Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3422,"ST",1,"MC",4.1020000000000003,1,"1FK70405AK711FB2"]
["1FK7040-5AK71-1TH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 1.6Nm, 100K, 6000rpm 0.69kW, Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1682,"ST",1,"MC",4.1020000000000003,1,"1FK70405AK711TH3"]
["1FK7042-2AC71-1CG2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.59kW; UDC=600V M0=3Nm (100K); NN=2000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without holding brake IP65 degree of protection DE flange IP67",2506,"ST",1,"MC",4.601,1,"1FK70422AC711CG2"]
["1FK7042-2AC74-1AA2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.59kW; UDC=600V M0=3Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1944,"ST",1,"MC",4.601,1,"1FK70422AC741AA2"]
["1FK7042-2AF21-1AB2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.82kW; UDC=300V; M0=3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2224,"ST",1,"MC",4.9000000000000004,1,"1FK70422AF211AB2"]
["1FK7042-2AF21-1UG2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.82kW; UDC=300V; M0=3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1482,"ST",1,"MC",4.6020000000000003,1,"1FK70422AF211UG2"]
["1FK7042-2AF71-1CB0","SIMOTICS S SIMOTICS S-1FK7 Synchronous motor 1FK7-CT PN=0.82k UDC=600V M0=3Nm (100K); NN=3000rpm; naturally cooled design MB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit + 12-bit multiturn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake, degree of protection IP64",2778,"ST",1,"MC",4.9000000000000004,1,"1FK70422AF711CB0"]
["1FK7042-2AF74-1AG2","SIMOTICS S SIMOTICS S-1FK7 Synchronous motor 1FK7-CT PN=0.82kW; UDC=600V M0=3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1852,"ST",1,"MC",4.601,1,"1FK70422AF741AG2"]
["1FK7042-2AF74-1TB2","SIMOTICS S SIMOTICS S-1FK7 Synchronous motor 1FK7-CT PN=0.82kW; UDC=600V M0=3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1596,"ST",1,"MC",4.9009999999999998,1,"1FK70422AF741TB2"]
["1FK7042-2AK71-1SB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.94kW; UDC=600V M0=3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1496,"ST",1,"MC",4.9009999999999998,1,"1FK70422AK711SB0"]
["1FK7042-2AK74-1EH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.94kW; UDC=600V M0=3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2427,"ST",1,"MC",4.9000000000000004,1,"1FK70422AK741EH0"]
["1FK7042-3BK71-1RH2","SIMOTICS S Synchronous motor 1FK7-HI PN=0.94kW; UDC=600V M0=3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2271,"ST",1,"MC",5.4,1,"1FK70423BK711RH2"]
["1FK7042-5AC71-1FG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, 3.0Nm 100K, 2000rpm, 0.59kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2931,"ST",1,"MC",4.9029999999999996,1,"1FK70425AC711FG0"]
["1FK7042-5AF21-1FB0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 3.0Nm, 100K 3000rpm, 0.82kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",3384,"ST",1,"MC",5.5019999999999998,1,"1FK70425AF211FB0"]
["1FK7042-5AF21-1KG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 3.0Nm, 100K 3000rpm, 0.82kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2255,"ST",1,"MC",4.9029999999999996,1,"1FK70425AF211KG0"]
["1FK7042-5AF21-1SG8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 3.0Nm, 100K 3000rpm, 0.82kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1681,"ST",1,"MC",4.9029999999999996,1,"1FK70425AF211SG8"]
["1FK7042-5AF71-1FB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 3.0Nm, 100K 3000rpm, 0.82kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",3384,"ST",1,"MC",5.5019999999999998,1,"1FK70425AF711FB0"]
["1FK7042-5AF71-1KH8","SIMOTICS S Synchronous servo motor 1FK7 Compact 3.0Nm, 100K 3000rpm, 0.82kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2905,"ST",1,"MC",5.5019999999999998,1,"1FK70425AF711KH8"]
["1FK7042-5AK71-1DB8","SIMOTICS S Synchronous servo motor 1FK7 Compact 3.0Nm, 100K, 6000rpm 1.02kW, Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3214,"ST",1,"MC",5.5019999999999998,1,"1FK70425AK711DB8"]
["1FK7042-5AK71-1FA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 3.0Nm, 100K, 6000rpm 1.02kW, Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3102,"ST",1,"MC",4.9029999999999996,1,"1FK70425AK711FA3"]
["1FK7042-5AK71-1UB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 3.0Nm, 100K, 6000rpm 1.02kW, Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER MULTI-POLE (RESOLVER P=4) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2196,"ST",1,"MC",5.5019999999999998,1,"1FK70425AK711UB3"]
["1FK7043-4CF21-1CB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.94kW; UDC=300V; M0=3. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2925,"ST",1,"MC",6.3,1,"1FK70434CF211CB1"]
["1FK7043-4CH71-1BB0","SIMOTICS S Synchronous motor 1FK7-HD PN=1.2kW; UDC=600V M0=3.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2429,"ST",1,"MC",6.3,1,"1FK70434CH711BB0"]
["1FK7043-4CH71-1QG2","SIMOTICS S Synchronous motor 1FK7-HD PN=1.2kW; UDC=600V M0=3.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1640,"ST",1,"MC",6.0010000000000003,1,"1FK70434CH711QG2"]
["1FK7043-4CK71-1AH2","SIMOTICS S Synchronous motor 1FK7-HD PN=1.3kW; UDC=600V M0=3.5Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2176,"ST",1,"MC",6.3,1,"1FK70434CK711AH2"]
["1FK7043-4CK71-1EB0","SIMOTICS S Synchronous motor 1FK7-HD PN=1.3kW; UDC=600V M0=3.5Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2569,"ST",1,"MC",6.3,1,"1FK70434CK711EB0"]
["1FK7043-7AF21-1AB5","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic, DC link 300V 3.1Nm, 100K, 3000 rpm 0.79kW, Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2826,"ST",1,"MC",6.9020000000000001,1,"1FK70437AF211AB5"]
["1FK7043-7AF21-1EA2","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic, DC link 300V 3.1Nm, 100K, 3000 rpm 0.79kW, Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2911,"ST",1,"MC",6.3029999999999999,1,"1FK70437AF211EA2"]
["1FK7043-7AF21-1TG8","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic, DC link 300V 3.1Nm, 100K, 3000 rpm 0.79kW, Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1738,"ST",1,"MC",6.3029999999999999,1,"1FK70437AF211TG8"]
["1FK7043-7AH71-1AB3","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic, 3.1Nm 100K, 4500rpm, 1.23kW Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2704,"ST",1,"MC",6.9020000000000001,1,"1FK70437AH711AB3"]
["1FK7043-7AH71-1GH3","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic, 3.1Nm 100K, 4500rpm, 1.23kW Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2398,"ST",1,"MC",6.9020000000000001,1,"1FK70437AH711GH3"]
["1FK7043-7AH71-1TG8","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic, 3.1Nm 100K, 4500rpm, 1.23kW Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1738,"ST",1,"MC",6.3029999999999999,1,"1FK70437AH711TG8"]
["1FK7043-7AK71-1GB0","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic 3.1Nm, 100K, 6000rpm 1.26kW, Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2454,"ST",1,"MC",6.9020000000000001,1,"1FK70437AK711GB0"]
["1FK7043-7AK71-1SA0","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic 3.1Nm, 100K, 6000rpm 1.26kW, Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1539,"ST",1,"MC",6.3029999999999999,1,"1FK70437AK711SA0"]
["1FK7043-7AK71-1TG5","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic 3.1Nm, 100K, 6000rpm 1.26kW, Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1608,"ST",1,"MC",6.3029999999999999,1,"1FK70437AK711TG5"]
["1FK7044-4CF71-1PG1","SIMOTICS S Synchronous motor 1FK7-HD PN=1.2kW; UDC=600V M0=4.5Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1605,"ST",1,"MC",7.5010000000000003,1,"1FK70444CF711PG1"]
["1FK7044-4CF74-1AA1","SIMOTICS S Synchronous motor 1FK7-HD PN=1.2kW; UDC=600V M0=4.5Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2067,"ST",1,"MC",7.4009999999999998,1,"1FK70444CF741AA1"]
["1FK7044-4CH71-1QA1","SIMOTICS S Synchronous motor 1FK7-HD PN=1.4kW; UDC=600V M0=4.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1808,"ST",1,"MC",7.4009999999999998,1,"1FK70444CH711QA1"]
["1FK7044-4CH71-1UG2","SIMOTICS S Synchronous motor 1FK7-HD PN=1.4kW; UDC=600V M0=4.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1605,"ST",1,"MC",7.4020000000000001,1,"1FK70444CH711UG2"]
["1FK7044-7AF71-1EH8","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic 4.0Nm, 100K 3000rpm, 1.1 kW Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3419,"ST",1,"MC",8.3019999999999996,1,"1FK70447AF711EH8"]
["1FK7044-7AF71-1GG3","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic 4.0Nm, 100K 3000rpm, 1.1 kW Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2153,"ST",1,"MC",7.7030000000000003,1,"1FK70447AF711GG3"]
["1FK7044-7AF71-1UH0","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic 4.0Nm, 100K 3000rpm, 1.1 kW Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2171,"ST",1,"MC",8.3019999999999996,1,"1FK70447AF711UH0"]
["1FK7044-7AH71-1EH8","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic, 4.0Nm 100K, 4500rpm, 1.41kW Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3419,"ST",1,"MC",8.3019999999999996,1,"1FK70447AH711EH8"]
["1FK7044-7AH71-1UG3","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic, 4.0Nm 100K, 4500rpm, 1.41kW Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1893,"ST",1,"MC",7.7030000000000003,1,"1FK70447AH711UG3"]
["1FK7060-2AC71-1CA1","SIMOTICS S Synchronous motor 1FK7-CT PN=1.1kW; UDC=600V M0=6Nm (100K); NN=2000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake IP65 degree of protection",2828,"ST",1,"MC",7.101,1,"1FK70602AC711CA1"]
["1FK7060-2AC71-1UG2","SIMOTICS S Synchronous motor 1FK7-CT PN=1.1kW; UDC=600V M0=6Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1712,"ST",1,"MC",7.1020000000000003,1,"1FK70602AC711UG2"]
["1FK7060-2AF71-1CH1","SIMOTICS S synchronous motor 1FK7-CT PN=1.5kW; UDC=600V M0=6Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit + 12-bit multiturn with DRIVE-CLiQ interface (encoder AM24DQI) Smooth shaft, tolerance N with holding brake, degree of protection IP65",3063,"ST",1,"MC",7.4,1,"1FK70602AF711CH1"]
["1FK7060-2AF71-1SB2","SIMOTICS S Synchronous motor 1FK7-CT PN=1.5kW; UDC=600V M0=6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1871,"ST",1,"MC",7.4009999999999998,1,"1FK70602AF711SB2"]
["1FK7060-2AF74-1AA0","SIMOTICS S Synchronous motor 1FK7-CT PN=1.5kW; UDC=600V M0=6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2074,"ST",1,"MC",7.101,1,"1FK70602AF741AA0"]
["1FK7060-2AH71-1AG0","SIMOTICS S Synchronous motor 1FK7-CT PN=1.7kW; UDC=600V M0=6Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1981,"ST",1,"MC",7.101,1,"1FK70602AH711AG0"]
["1FK7060-2AH71-1TH1","SIMOTICS S Synchronous motor 1FK7-CT PN=1.7kW; UDC=600V M0=6Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1781,"ST",1,"MC",7.4009999999999998,1,"1FK70602AH711TH1"]
["1FK7060-3BF71-1AB2","SIMOTICS S Synchronous motor 1FK7-HI PN=1.5kW; UDC=600V M0=6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VP 2048 S/R WITH C- AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2499,"ST",1,"MC",8.1,1,"1FK70603BF711AB2"]
["1FK7060-3BF74-1EG1","SIMOTICS S Synchronous motor 1FK7-HI PN=1.5kW; UDC=600V M0=6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2480,"ST",1,"MC",7.8010000000000002,1,"1FK70603BF741EG1"]
["1FK7060-5AF71-1DB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 6.0Nm, 100K 3000rpm, 1.48kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3418,"ST",1,"MC",8.3019999999999996,1,"1FK70605AF711DB5"]
["1FK7060-5AF71-1TA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 6.0Nm, 100K 3000rpm, 1.48kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1884,"ST",1,"MC",7.0030000000000001,1,"1FK70605AF711TA2"]
["1FK7060-5AF71-1UG8","SIMOTICS S Synchronous servo motor 1FK7 Compact 6.0Nm, 100K 3000rpm, 1.48kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER MULTI-POLE (RESOLVER P=4) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2275,"ST",1,"MC",7.0030000000000001,1,"1FK70605AF711UG8"]
["1FK7060-5AH71-1FG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 6.0Nm, 100K, 4500rpm 1.74kW, Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",3211,"ST",1,"MC",7.0030000000000001,1,"1FK70605AH711FG0"]
["1FK7060-5AH71-1SH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 6.0Nm, 100K, 4500rpm 1.74kW, Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2229,"ST",1,"MC",8.3019999999999996,1,"1FK70605AH711SH5"]
["1FK7061-4CF71-1QA0","SIMOTICS S Synchronous motor 1FK7-HD PN=1.7kW; UDC=600V M0=6.4Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1933,"ST",1,"MC",9.5009999999999994,1,"1FK70614CF711QA0"]
["1FK7061-4CF71-1UG1","SIMOTICS S Synchronous motor 1FK7-HD PN=1.7kW; UDC=600V M0=6.4Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1831,"ST",1,"MC",9.5020000000000007,1,"1FK70614CF711UG1"]
["1FK7061-4CH71-1PH1","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=6.4Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2158,"ST",1,"MC",9.9,1,"1FK70614CH711PH1"]
["1FK7061-4CH71-1SG1","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=6.4Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1572,"ST",1,"MC",9.5020000000000007,1,"1FK70614CH711SG1"]
["1FK7061-7AF71-1AA8","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic, 6.4Nm 100K, 3000rpm, 1.70kW Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2983,"ST",1,"MC",10.003,1,"1FK70617AF711AA8"]
["1FK7061-7AF71-1GG0","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic, 6.4Nm 100K, 3000rpm, 1.70kW Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2368,"ST",1,"MC",10.003,1,"1FK70617AF711GG0"]
["1FK7061-7AF71-1SB0","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic, 6.4Nm 100K, 3000rpm, 1.70kW Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2301,"ST",1,"MC",11.302,1,"1FK70617AF711SB0"]
["1FK7061-7AH71-1EH2","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic, 6.4Nm 100K, 4500rpm, 2.03kW Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3564,"ST",1,"MC",11.302,1,"1FK70617AH711EH2"]
["1FK7061-7AH71-1TB3","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic, 6.4Nm 100K, 4500rpm, 2.03kW Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2361,"ST",1,"MC",11.302,1,"1FK70617AH711TB3"]
["1FK7062-2AC71-1CG1","SIMOTICS S synchronous motor 1FK7-CT PN=1.5kW; UDC=600V M0=8.5Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit + 12-bit multiturn with DRIVE-CLiQ interface (encoder AM24DQI) Smooth shaft, tolerance N without holding brake, degree of protection IP65",2875,"ST",1,"MC",9.1010000000000009,1,"1FK70622AC711CG1"]
["1FK7062-2AC71-1EH2","SIMOTICS S Synchronous motor 1FK7-CT PN=1.5kW; UDC=600V M0=8.5Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2946,"ST",1,"MC",9.4,1,"1FK70622AC711EH2"]
["1FK7062-2AC74-1SH0","SIMOTICS S Synchronous motor 1FK7-CT PN=1.5kW; UDC=600V M0=8.5Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1820,"ST",1,"MC",9.4009999999999998,1,"1FK70622AC741SH0"]
["1FK7062-2AF71-1DH0","SIMOTICS S Synchronous motor 1FK7-CT PN=1.9kW; UDC=600V M0=8.5Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2792,"ST",1,"MC",9.4009999999999998,1,"1FK70622AF711DH0"]
["1FK7062-2AF74-1EG2","SIMOTICS S Synchronous motor 1FK7-CT PN=1.9kW; UDC=600V M0=8.5Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2619,"ST",1,"MC",9.1010000000000009,1,"1FK70622AF741EG2"]
["1FK7062-2AH71-1BG0","SIMOTICS S Synchronous motor 1FK7-CT PN=1.4kW; UDC=600V M0=8.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2379,"ST",1,"MC",9.1010000000000009,1,"1FK70622AH711BG0"]
["1FK7062-2AH74-1EA1","SIMOTICS S Synchronous motor 1FK7-CT PN=1.4kW; UDC=600V M0=8.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2711,"ST",1,"MC",9.1010000000000009,1,"1FK70622AH741EA1"]
["1FK7062-2AH74-1TH1","SIMOTICS S Synchronous motor 1FK7-CT PN=1.4kW; UDC=600V M0=8.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1920,"ST",1,"MC",9.4009999999999998,1,"1FK70622AH741TH1"]
["1FK7063-2AC71-1BG1","SIMOTICS S synchronous motor 1FK7-CT PN=1.9kW; UDC=600V M0=11Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) Smooth shaft, tolerance N without holding brake, degree of protection IP65",2579,"ST",1,"MC",11.101000000000001,1,"1FK70632AC711BG1"]
["1FK7063-2AC71-1EH0","SIMOTICS S Synchronous motor 1FK7-CT PN=1.9kW; UDC=600V M0=11Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2946,"ST",1,"MC",11.4,1,"1FK70632AC711EH0"]
["1FK7063-2AC71-1SH1","SIMOTICS S Synchronous motor 1FK7-CT PN=1.9kW; UDC=600V M0=11Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2020,"ST",1,"MC",11.401,1,"1FK70632AC711SH1"]
["1FK7063-2AF71-1DA0","SIMOTICS S Synchronous motor 1FK7-CT PN=2.3kW; UDC=600V M0=11Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2657,"ST",1,"MC",11.102,1,"1FK70632AF711DA0"]
["1FK7063-2AF74-1AA2","SIMOTICS S Synchronous motor 1FK7-CT PN=2.3kW; UDC=600V M0=11Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2413,"ST",1,"MC",11.101000000000001,1,"1FK70632AF741AA2"]
["1FK7063-2AH71-1AH0","SIMOTICS S Synchronous motor 1FK7-CT PN=1.4kW; UDC=600V M0=11Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2548,"ST",1,"MC",11.4,1,"1FK70632AH711AH0"]
["1FK7063-2AH71-1EA2","SIMOTICS S Synchronous motor 1FK7-CT PN=1.4kW; UDC=600V M0=11Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2812,"ST",1,"MC",11.101000000000001,1,"1FK70632AH711EA2"]
["1FK7063-2AH74-1EH2","SIMOTICS S Synchronous motor 1FK7-CT PN=1.4kW; UDC=600V M0=11Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3046,"ST",1,"MC",11.4,1,"1FK70632AH741EH2"]
["1FK7063-5AF71-1AH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 11Nm, 100K 3000rpm, 2.29kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",3104,"ST",1,"MC",12.802,1,"1FK70635AF711AH0"]
["1FK7063-5AF71-1PA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 11Nm, 100K 3000rpm, 2.29kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2549,"ST",1,"MC",11.503,1,"1FK70635AF711PA5"]
["1FK7063-5AF71-1TH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 11Nm, 100K 3000rpm, 2.29kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2520,"ST",1,"MC",12.802,1,"1FK70635AF711TH5"]
["1FK7063-5AH71-1GB8","SIMOTICS S Synchronous servo motor 1FK7 Compact, 11Nm 100K, 4500rpm, 1.41kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3335,"ST",1,"MC",12.802,1,"1FK70635AH711GB8"]
["1FK7063-5AH71-1PA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, 11Nm 100K, 4500rpm, 1.41kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2427,"ST",1,"MC",11.503,1,"1FK70635AH711PA3"]
["1FK7064-4CC71-1EB0","SIMOTICS S Synchronous motor 1FK7-HD PN=2.1kW; UDC=600V M0=12Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",3207,"ST",1,"MC",15.7,1,"1FK70644CC711EB0"]
["1FK7064-4CC71-1SA2","SIMOTICS S Synchronous motor 1FK7-HD PN=2.1kW; UDC=600V M0=12Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1956,"ST",1,"MC",15.401999999999999,1,"1FK70644CC711SA2"]
["1FK7064-4CF71-1CB2","SIMOTICS S Synchronous motor 1FK7-HD PN=2.5kW; UDC=600V M0=12Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3563,"ST",1,"MC",15.7,1,"1FK70644CF711CB2"]
["1FK7064-4CF71-1RB1","SIMOTICS S Synchronous motor 1FK7-HD PN=2.5kW; UDC=600V M0=12Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",3050,"ST",1,"MC",15.7,1,"1FK70644CF711RB1"]
["1FK7064-4CH71-1BG1","SIMOTICS S Synchronous motor 1FK7-HD PN=2.4kW; UDC=600V M0=12Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2750,"ST",1,"MC",15.401,1,"1FK70644CH711BG1"]
["1FK7064-4CH71-1EB2","SIMOTICS S Synchronous motor 1FK7-HD PN=2.4kW; UDC=600V M0=12Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3307,"ST",1,"MC",15.7,1,"1FK70644CH711EB2"]
["1FK7064-7AF71-1AG5","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic, 12.0Nm 100K, 3000rpm, 2.5kW Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3095,"ST",1,"MC",15.503,1,"1FK70647AF711AG5"]
["1FK7064-7AF71-1EB2","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic, 12.0Nm 100K, 3000rpm, 2.5kW Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",4028,"ST",1,"MC",16.802,1,"1FK70647AF711EB2"]
["1FK7064-7AF71-1KA2","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic, 12.0Nm 100K, 3000rpm, 2.5kW Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3269,"ST",1,"MC",15.503,1,"1FK70647AF711KA2"]
["1FK7064-7AH71-1AG3","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic 12.0Nm, 100K, 4500rpm 2.36kW, Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2972,"ST",1,"MC",15.503,1,"1FK70647AH711AG3"]
["1FK7064-7AH71-1GH3","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic 12.0Nm, 100K, 4500rpm 2.36kW, Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3180,"ST",1,"MC",16.802,1,"1FK70647AH711GH3"]
["1FK7064-7AH71-1TH8","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic 12.0Nm, 100K, 4500rpm 2.36kW, Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2858,"ST",1,"MC",16.802,1,"1FK70647AH711TH8"]
["1FK7080-2AF71-1BA0","SIMOTICS S Synchronous motor 1FK7-CT PN=2.1kW; UDC=600V M0=8Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2515,"ST",1,"MC",10.301,1,"1FK70802AF711BA0"]
["1FK7080-2AF74-1EA1","SIMOTICS S Synchronous motor 1FK7-CT PN=2.1kW; UDC=600V M0=8Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2755,"ST",1,"MC",10.301,1,"1FK70802AF741EA1"]
["1FK7080-2AF74-1TH1","SIMOTICS S Synchronous motor 1FK7-CT PN=2.1kW; UDC=600V M0=8Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2077,"ST",1,"MC",10.601000000000001,1,"1FK70802AF741TH1"]
["1FK7080-2AH71-1TH0","SIMOTICS S Synchronous motor 1FK7-CT PN=2.1kW; UDC=600V M0=8Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1977,"ST",1,"MC",10.601000000000001,1,"1FK70802AH711TH0"]
["1FK7080-2AH74-1EH1","SIMOTICS S Synchronous motor 1FK7-CT PN=2.1kW; UDC=600V M0=8Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",3103,"ST",1,"MC",10.6,1,"1FK70802AH741EH1"]
["1FK7080-5AF71-1KA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 8Nm, 100K, 3000rpm, 2.14kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N, WITHOUT HOLDING BRAKE; DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3051,"ST",1,"MC",10.003,1,"1FK70805AF711KA5"]
["1FK7080-5AF71-1SH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 8Nm, 100K, 3000rpm, 2.14kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N WITH HOLDING BRAKE; DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2509,"ST",1,"MC",12.502000000000001,1,"1FK70805AF711SH5"]
["1FK7080-5AH71-1FB8","SIMOTICS S Synchronous servo motor 1FK7 Compact, 8Nm 100K, 4500rpm, 2.10kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N, WITH HOLDING BRAKE; DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",4313,"ST",1,"MC",12.502000000000001,1,"1FK70805AH711FB8"]
["1FK7080-5AH71-1KA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, 8Nm 100K, 4500rpm, 2.10kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N, WITHOUT HOLDING BRAKE; DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2929,"ST",1,"MC",10.003,1,"1FK70805AH711KA3"]
["1FK7081-2AC71-1AA0","SIMOTICS S Synchronous motor 1FK7-CT PN=2.1kW; UDC=600V M0=12Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2489,"ST",1,"MC",12.901,1,"1FK70812AC711AA0"]
["1FK7081-2AC71-1PH2","SIMOTICS S Synchronous motor 1FK7-CT PN=2.1kW; UDC=600V M0=12Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE Smooth shaft, tolerance N With holding brake PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2568,"ST",1,"MC",13.3,1,"1FK70812AC711PH2"]
["1FK7081-2AF71-1AA2","SIMOTICS S Synchronous motor 1FK7-CT PN=2.7kW; UDC=600V M0=12Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2590,"ST",1,"MC",12.901,1,"1FK70812AF711AA2"]
["1FK7081-2AF71-1PA1","SIMOTICS S Synchronous motor 1FK7-CT PN=2.7kW; UDC=600V M0=12Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2220,"ST",1,"MC",13.000999999999999,1,"1FK70812AF711PA1"]
["1FK7081-2AF74-1TB1","SIMOTICS S Synchronous motor 1FK7-CT PN=2.7kW; UDC=600V M0=12Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2402,"ST",1,"MC",13.201000000000001,1,"1FK70812AF741TB1"]
["1FK7081-2AH71-1QH1","SIMOTICS S Synchronous motor 1FK7-CT PN=1.8kW; UDC=600V M0=12Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) Smooth shaft, tolerance N With holding brake PROTECTION CLASS IP65,",2679,"ST",1,"MC",13.2,1,"1FK70812AH711QH1"]
["1FK7081-2AH71-1RG0","SIMOTICS S Synchronous motor 1FK7-CT PN=1.8kW; UDC=600V M0=12Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2539,"ST",1,"MC",12.901,1,"1FK70812AH711RG0"]
["1FK7081-3BF71-1BH0","SIMOTICS S synchronous motor 1FK7-HI PN=2.7kW; UDC=600V M0=12Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) Smooth shaft, tolerance N with holding brake, degree of protection IP64",3096,"ST",1,"MC",15.5,1,"1FK70813BF711BH0"]
["1FK7081-3BF71-1RA0","SIMOTICS S synchronous motor 1FK7-HI PN=2.7kW; UDC=600V M0=12Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 20-bit + 12-bit multiturn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake, degree of protection IP64",2631,"ST",1,"MC",15.201000000000001,1,"1FK70813BF711RA0"]
["1FK7083-2AC71-1AH0","SIMOTICS S Synchronous motor 1FK7-CT PN=2.6kW; UDC=600V M0=16Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2953,"ST",1,"MC",15.9,1,"1FK70832AC711AH0"]
["1FK7083-2AC71-1PG0","SIMOTICS S Synchronous motor 1FK7-CT PN=2.6kW; UDC=600V M0=16Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2143,"ST",1,"MC",15.701000000000001,1,"1FK70832AC711PG0"]
["1FK7083-2AC74-1EH2","SIMOTICS S Synchronous motor 1FK7-CT PN=2.6kW; UDC=600V M0=16Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3451,"ST",1,"MC",15.9,1,"1FK70832AC741EH2"]
["1FK7083-2AF71-1CG1","SIMOTICS S synchronous motor 1FK7-CT PN=3.3kW; UDC=600V M0=16Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit + 12-bit multiturn with DRIVE-CLiQ interface (encoder AM24DQI) Smooth shaft, tolerance N without holding brake, degree of protection IP65",3266,"ST",1,"MC",15.601000000000001,1,"1FK70832AF711CG1"]
["1FK7083-2AF74-1EG0","SIMOTICS S Synchronous motor 1FK7-CT PN=3.3kW; UDC=600V M0=16Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2910,"ST",1,"MC",15.601000000000001,1,"1FK70832AF741EG0"]
["1FK7083-2AH71-1AB0","SIMOTICS S Synchronous motor 1FK7-CT PN=1.4kW; UDC=600V M0=16Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",3045,"ST",1,"MC",15.9,1,"1FK70832AH711AB0"]
["1FK7083-2AH71-1TG0","SIMOTICS S Synchronous motor 1FK7-CT PN=1.4kW; UDC=600V M0=16Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1884,"ST",1,"MC",15.602,1,"1FK70832AH711TG0"]
["1FK7083-5AC71-1KG5","SIMOTICS S Synchronous servo motor 1FK7 COMPACT 16Nm, 100K 2000rpm, 2.62kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3363,"ST",1,"MC",14.003,1,"1FK70835AC711KG5"]
["1FK7083-5AF71-1FA8","SIMOTICS S Synchronous servo motor 1FK7 COMPACT 16Nm, 100K 3000rpm, 3.30kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",4282,"ST",1,"MC",14.003,1,"1FK70835AF711FA8"]
["1FK7083-5AF71-1KH8","SIMOTICS S Synchronous servo motor 1FK7 COMPACT 16Nm, 100K 3000rpm, 3.30kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",4031,"ST",1,"MC",16.501999999999999,1,"1FK70835AF711KH8"]
["1FK7083-5AH71-1DB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, 16Nm 100K, 4500rpm, 3.04kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",4084,"ST",1,"MC",16.501999999999999,1,"1FK70835AH711DB3"]
["1FK7083-5AH71-1FA0","SIMOTICS S Synchronous servo motor 1FK7 Compact, 16Nm 100K, 4500rpm, 3.04kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",3970,"ST",1,"MC",14.003,1,"1FK70835AH711FA0"]
["1FK7083-5AH71-1PH2","SIMOTICS S Synchronous servo motor 1FK7 Compact, 16Nm 100K, 4500rpm, 3.04kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3269,"ST",1,"MC",16.501999999999999,1,"1FK70835AH711PH2"]
["1FK7084-2AC71-1CA2","SIMOTICS S Synchronous motor 1FK7-CT PN=3.1kW; UDC=600V M0=20Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3678,"ST",1,"MC",18.300999999999998,1,"1FK70842AC711CA2"]
["1FK7084-2AC74-1AA0","SIMOTICS S Synchronous motor 1FK7-CT PN=3.1kW; UDC=600V M0=20Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2924,"ST",1,"MC",18.300999999999998,1,"1FK70842AC741AA0"]
["1FK7084-2AF71-1AG1","SIMOTICS S Synchronous motor 1FK7-CT PN=3.1kW; UDC=600V M0=20Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2932,"ST",1,"MC",18.300999999999998,1,"1FK70842AF711AG1"]
["1FK7084-2AF71-1DG0","SIMOTICS S Synchronous motor 1FK7-CT PN=3.1kW; UDC=600V M0=20Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3176,"ST",1,"MC",18.302,1,"1FK70842AF711DG0"]
["1FK7084-2AF74-1TH1","SIMOTICS S Synchronous motor 1FK7-CT PN=3.1kW; UDC=600V M0=20Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); Smooth shaft, tolerance N With holding brake PROTECTION CLASS IP65,",2744,"ST",1,"MC",18.600999999999999,1,"1FK70842AF741TH1"]
["1FK7084-3BC71-1CB1","SIMOTICS S synchronous motor 1FK7-HI PN=3.1kW; UDC=600V M0=20Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit + 12-bit multiturn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake, degree of protection IP65",4119,"ST",1,"MC",23,1,"1FK70843BC711CB1"]
["1FK7084-3BF71-1CA0","SIMOTICS S Synchronous motor 1FK7-HI PN=3.1kW; UDC=600V M0=20Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3578,"ST",1,"MC",22.701000000000001,1,"1FK70843BF711CA0"]
["1FK7084-3BF71-1QH1","SIMOTICS S Synchronous motor 1FK7-HI PN=3.1kW; UDC=600V M0=20Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) Smooth shaft, tolerance N With holding brake PROTECTION CLASS IP65,",3113,"ST",1,"MC",23,1,"1FK70843BF711QH1"]
["1FK7085-4CC71-1RA1","SIMOTICS S Synchronous motor 1FK7-HD PN=3.1kW; UDC=600V M0=22Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",3316,"ST",1,"MC",23.001000000000001,1,"1FK70854CC711RA1"]
["1FK7085-4CC74-1AG2","SIMOTICS S Synchronous motor 1FK7-HD PN=3.1kW; UDC=600V M0=22Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3082,"ST",1,"MC",23.001000000000001,1,"1FK70854CC741AG2"]
["1FK7085-4CF71-1CB0","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=22Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",4169,"ST",1,"MC",23.3,1,"1FK70854CF711CB0"]
["1FK7085-4CF71-1TA2","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=22Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2546,"ST",1,"MC",23.001999999999999,1,"1FK70854CF711TA2"]
["1FK7085-4CF74-1SH0","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=22Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2794,"ST",1,"MC",23.300999999999998,1,"1FK70854CF741SH0"]
["1FK7085-7AF71-1GH2","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic 22Nm 100K, 3000rpm, 3.14kW Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",4101,"ST",1,"MC",26.001999999999999,1,"1FK70857AF711GH2"]
["1FK7086-4CC71-1AG0","SIMOTICS S Synchronous motor 1FK7-HD PN=3.8kW; UDC=600V M0=28Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3408,"ST",1,"MC",23.001000000000001,1,"1FK70864CC711AG0"]
["1FK7086-4CC71-1RB0","SIMOTICS S Synchronous motor 1FK7-HD PN=3.8kW; UDC=600V M0=28Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",4083,"ST",1,"MC",23.3,1,"1FK70864CC711RB0"]
["1FK7086-4CF71-1AA2","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=28Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3601,"ST",1,"MC",23.001000000000001,1,"1FK70864CF711AA2"]
["1FK7086-4CF71-1PG0","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=28Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3038,"ST",1,"MC",23.100999999999999,1,"1FK70864CF711PG0"]
["1FK7086-4CF71-1SB0","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=28Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",3313,"ST",1,"MC",23.300999999999998,1,"1FK70864CF711SB0"]
["1FK7086-7AC71-1GA3","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic, 28Nm 100K, 2000rpm, 3.77kW Naturally cooled power/signal connectors Connector can be rotated by 270Β° IM B5 (V1, V3) BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",4133,"ST",1,"MC",23.503,1,"1FK70867AC711GA3"]
["1FK7086-7AF71-1EG2","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic, 28Nm 100K, 3000rpm, 3.77kW Naturally cooled power/signal connectors Connector can be rotated by 270Β° IM B5 (V1, V3) ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",4759,"ST",1,"MC",23.503,1,"1FK70867AF711EG2"]
["1FK7086-7AF71-1TA8","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic, 28Nm 100K, 3000rpm, 3.77kW Naturally cooled power/signal connectors Connector can be rotated by 270Β° IM B5 (V1, V3) RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3811,"ST",1,"MC",23.503,1,"1FK70867AF711TA8"]
["1FK7086-7SF71-1EG0","SIMOTICS S Synchronous servo motor 1FK7 High Dynamic, 38Nm 100K, 3000rpm, 7.50kW Forced ventilation IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° IM B5 (V1, V3) ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",6282,"ST",1,"MC",27.603000000000002,1,"1FK70867SF711EG0"]
["1FK7100-2AC71-1PH2","SIMOTICS S Synchronous motor 1FK7-CT PN=3kW; UDC=600V M0=18Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2949,"ST",1,"MC",18,1,"1FK71002AC711PH2"]
["1FK7100-2AC71-1SG2","SIMOTICS S Synchronous motor 1FK7-CT PN=3kW; UDC=600V M0=18Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2250,"ST",1,"MC",17.602,1,"1FK71002AC711SG2"]
["1FK7100-2AF71-1DG0","SIMOTICS S Synchronous motor 1FK7-CT PN=3.8kW; UDC=600V M0=18Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3122,"ST",1,"MC",17.602,1,"1FK71002AF711DG0"]
["1FK7100-2AF71-1RG0","SIMOTICS S Synchronous motor 1FK7-CT PN=3.8kW; UDC=600V M0=18Nm (100K); NN=3000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 20-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without holding brake IP64 degree of protection",2919,"ST",1,"MC",17.600999999999999,1,"1FK71002AF711RG0"]
["1FK7100-3BC71-1CH0","SIMOTICS S Synchronous motor 1FK7-HI PN=3kW; UDC=600V M0=18Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",3863,"ST",1,"MC",19.7,1,"1FK71003BC711CH0"]
["1FK7100-5AC71-1DA0","SIMOTICS S Synchronous servo motor 1FK7 Compact, 18Nm 100K, 2000rpm, 3.05kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",3811,"ST",1,"MC",19.003,1,"1FK71005AC711DA0"]
["1FK7100-5AF71-1FH8","SIMOTICS S Synchronous servo motor 1FK7 Compact, 18Nm 100K, 3000rpm, 3.77kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",5029,"ST",1,"MC",22.001999999999999,1,"1FK71005AF711FH8"]
["1FK7100-5AF71-1PG8","SIMOTICS S Synchronous servo motor 1FK7 Compact, 18Nm 100K, 3000rpm, 3.77kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3245,"ST",1,"MC",19.003,1,"1FK71005AF711PG8"]
["1FK7100-5AF71-1TH8","SIMOTICS S Synchronous servo motor 1FK7 Compact, 18Nm 100K, 3000rpm, 3.77kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3468,"ST",1,"MC",22.001999999999999,1,"1FK71005AF711TH8"]
["1FK7101-2AC71-1QA1","SIMOTICS S Synchronous motor 1FK7-CT PN=4.3kW; UDC=600V M0=27Nm (100K); NN=2000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake IP65 degree of protection",3055,"ST",1,"MC",23.001000000000001,1,"1FK71012AC711QA1"]
["1FK7101-2AC71-1UG2","SIMOTICS S Synchronous motor 1FK7-CT PN=4.3kW; UDC=600V M0=27Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2852,"ST",1,"MC",23.001999999999999,1,"1FK71012AC711UG2"]
["1FK7101-2AF71-1FA2","SIMOTICS S Synchronous motor 1FK7-CT PN=4.9kW; UDC=600V M0=27Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",4054,"ST",1,"MC",23.001000000000001,1,"1FK71012AF711FA2"]
["1FK7101-2AF71-1RB1","SIMOTICS S synchronous motor 1FK7-CT PN=4.9kW; UDC=600V M0=27Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 20-bit + 12-bit multiturn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake, degree of protection IP65",3896,"ST",1,"MC",23.3,1,"1FK71012AF711RB1"]
["1FK7101-3BC71-1QH1","SIMOTICS S synchronous motor 1FK7-HI PN=4.3kW; UDC=600V M0=27Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) Smooth shaft, tolerance N with holding brake, degree of protection IP65",3389,"ST",1,"MC",26,1,"1FK71013BC711QH1"]
["1FK7101-3BF71-1BA1","SIMOTICS S Synchronous motor 1FK7-HI PN=4.9kW; UDC=600V M0=27Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",3558,"ST",1,"MC",25.701000000000001,1,"1FK71013BF711BA1"]
["1FK7101-5AC71-1FA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, 27Nm 100K, 2000rpm, 4.29kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",4771,"ST",1,"MC",21.003,1,"1FK71015AC711FA3"]
["1FK7101-5AC71-1GH0","SIMOTICS S Synchronous servo motor 1FK7 Compact, 27Nm 100K, 2000rpm, 4.29kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",4149,"ST",1,"MC",24.001999999999999,1,"1FK71015AC711GH0"]
["1FK7101-5AF71-1AB2","SIMOTICS S Synchronous servo motor 1FK7 Compact, 27Nm 100K, 3000rpm, 4.85kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",4574,"ST",1,"MC",24.001999999999999,1,"1FK71015AF711AB2"]
["1FK7101-5AF71-1DH5","SIMOTICS S Synchronous servo motor 1FK7 Compact, 27Nm 100K, 3000rpm, 4.85kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",4835,"ST",1,"MC",24.001999999999999,1,"1FK71015AF711DH5"]
["1FK7101-5AF71-1TG5","SIMOTICS S Synchronous servo motor 1FK7 Compact, 27Nm 100K, 3000rpm, 4.85kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3219,"ST",1,"MC",21.003,1,"1FK71015AF711TG5"]
["1FK7103-2AC71-1CB1","SIMOTICS S Synchronous motor 1FK7-CT PN=5.2kW; UDC=600V M0=36Nm (100K); NN=2000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake IP65 degree of protection",4861,"ST",1,"MC",28.8,1,"1FK71032AC711CB1"]
["1FK7103-2AC74-1AG1","SIMOTICS S Synchronous motor 1FK7-CT PN=5.2kW; UDC=600V M0=36Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",3674,"ST",1,"MC",28.501000000000001,1,"1FK71032AC741AG1"]
["1FK7103-2AC74-1TB1","SIMOTICS S Synchronous motor 1FK7-CT PN=5.2kW; UDC=600V M0=36Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",3579,"ST",1,"MC",28.800999999999998,1,"1FK71032AC741TB1"]
["1FK7103-2AF71-1QH1","SIMOTICS S Synchronous motor 1FK7-CT PN=4.4kW; UDC=600V M0=36Nm (100K); NN=3000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with holding brake IP65 degree of protection",3856,"ST",1,"MC",28.8,1,"1FK71032AF711QH1"]
["1FK7103-2AF74-1SA0","SIMOTICS S Synchronous motor 1FK7-CT PN=4.4kW; UDC=600V M0=36Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3038,"ST",1,"MC",28.501999999999999,1,"1FK71032AF741SA0"]
["1FK7103-3BF71-1CA0","SIMOTICS S Synchronous motor 1FK7-HI PN=4.4kW; UDC=600V M0=36Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",4302,"ST",1,"MC",32.100999999999999,1,"1FK71033BF711CA0"]
["1FK7103-3BF74-1EG0","SIMOTICS S Synchronous motor 1FK7-HI PN=4.4kW; UDC=600V M0=36Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3954,"ST",1,"MC",32.100999999999999,1,"1FK71033BF741EG0"]
["1FK7103-5AC71-1DB3","SIMOTICS S Synchronous servo motor 1FK7 compact, 36Nm 100K, 2000rpm, 5.24kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",5377,"ST",1,"MC",32.002000000000002,1,"1FK71035AC711DB3"]
["1FK7103-5AC71-1TA0","SIMOTICS S Synchronous servo motor 1FK7 compact, 36Nm 100K, 2000rpm, 5.24kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",3701,"ST",1,"MC",29.003,1,"1FK71035AC711TA0"]
["1FK7103-5AC71-1UA5","SIMOTICS S Synchronous servo motor 1FK7 compact, 36Nm 100K, 2000rpm, 5.24kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER MULTI-POLE (RESOLVER P=4) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",4197,"ST",1,"MC",29.003,1,"1FK71035AC711UA5"]
["1FK7103-5AF71-1KB0","SIMOTICS S Synchronous servo motor 1FK7 compact, 36Nm 100K, 3000rpm, 4.40kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",5125,"ST",1,"MC",32.002000000000002,1,"1FK71035AF711KB0"]
["1FK7103-5AF71-1TA0","SIMOTICS S Synchronous servo motor 1FK7 compact, 36Nm 100K, 3000rpm, 4.40kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",3701,"ST",1,"MC",29.003,1,"1FK71035AF711TA0"]
["1FK7105-2AC71-1PB0","SIMOTICS S Synchronous motor 1FK7-CT PN=7.7kW; UDC=600V M0=48Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",4875,"ST",1,"MC",39.4,1,"1FK71052AC711PB0"]
["1FK7105-2AC71-1TH1","SIMOTICS S Synchronous motor 1FK7-CT PN=7.7kW; UDC=600V M0=48Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",4624,"ST",1,"MC",39.301000000000002,1,"1FK71052AC711TH1"]
["1FK7105-2AF71-1BH0","SIMOTICS S Synchronous motor 1FK7-CT PN=8.2kW; UDC=600V M0=48Nm (100K); NN=3000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with holding brake IP64 degree of protection",5410,"ST",1,"MC",39.299999999999997,1,"1FK71052AF711BH0"]
["1FK7105-2AF71-1QB1","SIMOTICS S Synchronous motor 1FK7-CT PN=8.2kW; UDC=600V M0=48Nm (100K); NN=3000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake IP65 degree of protection",5085,"ST",1,"MC",39.299999999999997,1,"1FK71052AF711QB1"]
["1FK7105-3BC71-1QA0","SIMOTICS S synchronous motor 1FK7-HI PN=7.7kW; UDC=600V M0=48Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake, degree of protection IP64",4517,"ST",1,"MC",44.401000000000003,1,"1FK71053BC711QA0"]
["1FK7105-3BC74-1AH0","SIMOTICS S Synchronous motor 1FK7-HI PN=7.7kW; UDC=600V M0=48Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VP 2048 S/R WITH C- AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",5124,"ST",1,"MC",44.7,1,"1FK71053BC741AH0"]
["1FK7105-5AC71-1GH2","SIMOTICS S Synchronous servo motor 1FK7 compact, 48Nm 100K, 2000rpm, 7.75kW Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",6208,"ST",1,"MC",42.101999999999997,1,"1FK71055AC711GH2"]
["1FK7105-5AC71-1UB0","SIMOTICS S Synchronous servo motor 1FK7 compact, 48Nm 100K, 2000rpm, 7.75kW Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER MULTI-POLE (RESOLVER P=4) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",5939,"ST",1,"MC",42.101999999999997,1,"1FK71055AC711UB0"]
["1FK7105-5AF71-1FA2","SIMOTICS S Synchronous servo motor 1FK7 compact, 48Nm 100K, 3000rpm, 8.17kW Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",6771,"ST",1,"MC",39.103000000000002,1,"1FK71055AF711FA2"]
["1FK7105-5AF71-1KH2","SIMOTICS S Synchronous servo motor 1FK7 compact, 48Nm 100K, 3000rpm, 8.17kW Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",6520,"ST",1,"MC",42.101999999999997,1,"1FK71055AF711KH2"]
["1FK7105-5AF71-1SB8","SIMOTICS S Synchronous servo motor 1FK7 compact, 48Nm 100K, 3000rpm, 8.17kW Naturally cooled IM B5 (V1, V3) power/signal connectors Connector can be rotated by 270Β° RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",5936,"ST",1,"MC",42.101999999999997,1,"1FK71055AF711SB8"]
["1FL6044-2AF21-1MA1","SIMOTICS S-1FL6 voltage supply 230 V 3AC Pn=1 kW; Nn=3000 rpm M0=3.18 Nm; MN=3.18 Nm. Shaft height 40 mm absolute encoder Single-turn 21-bit with feather key Tolerance N without holding brake Degree of protection IP65 with fitting oil seal for drive SINAMICS V90",866,"ST",1,"MC",3.39,1,"1FL60442AF211MA1"]
["1FL6092-1AC61-2AH1","SIMOTICS S-1FL6-1FL6 Operating voltage 3AC 400 V Pn=3.5 kW; Nn=2000 rpm M0=22 Nm; MN=16.7 Nm Shaft height 90 mm, with angle plug; incremental encoder 2500 incr./rev. plain shaft, Tolerance N with holding brake Degree of protection IP65 with sealing ring compatible with the converters SINAMICS V70 & V90",2213,"ST",1,"MC",28.25,1,"1FL60921AC612AH1"]
["1FT7034-5AK70-1FG1","SIMOTICS S Synchronous motor 1FT7, M0=2Nm (100K) NN=6000rpm, PN=0.88kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4327,"ST",1,"MC",3.9039999999999999,1,"1FT70345AK701FG1"]
["1FT7034-5AK71-1BK4","SIMOTICS S Synchronous motor 1FT7, M0=2Nm (100K) NN=6000rpm, PN=0.88kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",3759,"ST",1,"MC",3.9039999999999999,1,"1FT70345AK711BK4"]
["1FT7036-5AK70-1CA3","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=6000rpm, PN=1.07kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",4453,"ST",1,"MC",5.1040000000000001,1,"1FT70365AK701CA3"]
["1FT7036-5AK70-1FG2","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=6000rpm, PN=1.07kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",4561,"ST",1,"MC",5.1040000000000001,1,"1FT70365AK701FG2"]
["1FT7042-5AF70-1CK5","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=3000rpm, PN=0.85kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",4858,"ST",1,"MC",4.7039999999999997,1,"1FT70425AF701CK5"]
["1FT7042-5AF71-1CB1","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=3000rpm, PN=0.85kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",5170,"ST",1,"MC",5.4029999999999996,1,"1FT70425AF711CB1"]
["1FT7042-5AF71-1FK0","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=3000rpm, PN=0.85kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",4589,"ST",1,"MC",4.7039999999999997,1,"1FT70425AF711FK0"]
["1FT7042-5AK70-1CG1","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=6000rpm, PN=1.26kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4435,"ST",1,"MC",4.7039999999999997,1,"1FT70425AK701CG1"]
["1FT7042-5AK71-1LG1","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=6000rpm, PN=1.26kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) AND M17-CONNECTOR PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4757,"ST",1,"MC",4.7039999999999997,1,"1FT70425AK711LG1"]
["1FT7044-5AF70-1BA1","SIMOTICS S Synchronous motor 1FT7, M0=5Nm (100K) NN=3000rpm, PN=1.35kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4004,"ST",1,"MC",7.3040000000000003,1,"1FT70445AF701BA1"]
["1FT7044-5AF70-1FH4","SIMOTICS S Synchronous motor 1FT7, M0=5Nm (100K) NN=3000rpm, PN=1.35kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",5811,"ST",1,"MC",8.0030000000000001,1,"1FT70445AF701FH4"]
["1FT7044-5AF71-1FA2","SIMOTICS S Synchronous motor 1FT7, M0=5Nm (100K) NN=3000rpm, PN=1.35kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",4995,"ST",1,"MC",7.3040000000000003,1,"1FT70445AF711FA2"]
["1FT7044-5AF71-1NK5","SIMOTICS S Synchronous motor 1FT7, M0=5Nm (100K) NN=3000rpm, PN=1.35kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",4062,"ST",1,"MC",7.3040000000000003,1,"1FT70445AF711NK5"]
["1FT7044-5AK71-1DG2","SIMOTICS S Synchronous motor 1FT7, M0=5Nm (100K) NN=6000rpm, PN=1.41kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",4175,"ST",1,"MC",7.3040000000000003,1,"1FT70445AK711DG2"]
["1FT7046-5AF70-1FB0","SIMOTICS S Synchronous motor 1FT7, M0=7Nm (100K) NN=3000rpm, PN=1.76kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5868,"ST",1,"MC",10.103,1,"1FT70465AF701FB0"]
["1FT7046-5AF71-1DB1","SIMOTICS S Synchronous motor 1FT7, M0=7Nm (100K) NN=3000rpm, PN=1.76kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",5151,"ST",1,"MC",10.103,1,"1FT70465AF711DB1"]
["1FT7046-5AF71-1FH0","SIMOTICS S Synchronous motor 1FT7, M0=7Nm (100K) NN=3000rpm, PN=1.76kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5868,"ST",1,"MC",10.103,1,"1FT70465AF711FH0"]
["1FT7046-5AH74-1MH0","SIMOTICS S Synchronous motor 1FT7, M0=7Nm (100K) NN=4500rpm, PN=1.32kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with Pt1000 temperature sensor POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5406,"ST",1,"MC",10.103,1,"1FT70465AH741MH0"]
["1FT7062-1AK70-1FG1","SIMOTICS S Synchronous motor 1FT7, M0=6Nm (100K) NN=6000rpm, PN=2.13kW naturally cooled; Power connector rotatable; Vibration severity A Degree of protection IP65 Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACCURACY TOLERANCE N",3913,"ST",1,"MC",7.1,1,"1FT70621AK701FG1"]
["1FT7062-5AF71-1DA1","SIMOTICS S Synchronous motor 1FT7, M0=6Nm (100K) NN=3000rpm, PN=1.70kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4033,"ST",1,"MC",7.2039999999999997,1,"1FT70625AF711DA1"]
["1FT7062-5AF71-1NB0","SIMOTICS S Synchronous motor 1FT7, M0=6Nm (100K) NN=3000rpm, PN=1.70kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",4330,"ST",1,"MC",8.5030000000000001,1,"1FT70625AF711NB0"]
["1FT7062-5AK71-1FA1","SIMOTICS S Synchronous motor 1FT7, M0=6Nm (100K) NN=6000rpm, PN=2.13kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE Absolute encoder 22-bit Multiturn with DRIVE-CLiQ interface (encoder AM22DQ) Rotatable connector SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4853,"ST",1,"MC",7.2039999999999997,1,"1FT70625AK711FA1"]
["1FT7062-5WK70-1FH0","SIMOTICS S Synchronous motor 1FT7, M0=10Nm (100K) NN=6000rpm, PN=5.80kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE Absolute encoder 22-bit Multiturn with DRIVE-CLiQ interface (encoder AM22DQ) Rotatable connector PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6292,"ST",1,"MC",12.403,1,"1FT70625WK701FH0"]
["1FT7064-5AF70-1DA0","SIMOTICS S Synchronous motor 1FT7, M0=9Nm (100K) NN=3000rpm, PN=2.39kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",4385,"ST",1,"MC",9.8040000000000003,1,"1FT70645AF701DA0"]
["1FT7064-5AF70-1NA2","SIMOTICS S Synchronous motor 1FT7, M0=9Nm (100K) NN=3000rpm, PN=2.39kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact), with KTY  temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",4122,"ST",1,"MC",9.8040000000000003,1,"1FT70645AF701NA2"]
["1FT7064-5AF71-1DA2","SIMOTICS S Synchronous motor 1FT7, M0=9Nm (100K) NN=3000rpm, PN=2.39kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",4573,"ST",1,"MC",9.8040000000000003,1,"1FT70645AF711DA2"]
["1FT7064-5AK71-1CK5","SIMOTICS S Synchronous motor 1FT7, M0=9Nm (100K) NN=6000rpm, PN=2.59kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",5645,"ST",1,"MC",9.8040000000000003,1,"1FT70645AK711CK5"]
["1FT7064-5WF71-1FL4","SIMOTICS S Synchronous motor 1FT7, M0=16Nm (100K) NN=3000rpm, PN=5.00kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE Absolute encoder 22-bit Multiturn with DRIVE-CLiQ interface (encoder AM22DQ) Rotatable connector PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",7181,"ST",1,"MC",15.103,1,"1FT70645WF711FL4"]
["1FT7065-7SF70-1BA0","SIMOTICS S Synchronous motor 1FT7, M0=14Nm (100K) NN=3000rpm, PN=3.80kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5373,"ST",1,"MC",19.004000000000001,1,"1FT70657SF701BA0"]
["1FT7065-7WF70-1BG0","SIMOTICS S Synchronous motor 1FT7, M0=19Nm (100K) NN=3000rpm, PN=5.70kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5373,"ST",1,"MC",16.103999999999999,1,"1FT70657WF701BG0"]
["1FT7066-5AF71-1DB3","SIMOTICS S Synchronous motor 1FT7, M0=12Nm (100K) NN=3000rpm, PN=2.92kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",5733,"ST",1,"MC",13.702999999999999,1,"1FT70665AF711DB3"]
["1FT7066-5AF71-1NA0","SIMOTICS S Synchronous motor 1FT7, M0=12Nm (100K) NN=3000rpm, PN=2.92kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",4266,"ST",1,"MC",12.404,1,"1FT70665AF711NA0"]
["1FT7066-5AH71-1FH1","SIMOTICS S Synchronous motor 1FT7, M0=12Nm (100K) NN=4500rpm, PN=2.55kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE Absolute encoder 22-bit Multiturn with DRIVE-CLiQ interface (encoder AM22DQ) Rotatable connector PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6490,"ST",1,"MC",13.702999999999999,1,"1FT70665AH711FH1"]
["1FT7066-5WH70-1FG2","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=4500rpm, PN=9.10kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE Absolute encoder 22-bit Multiturn with DRIVE-CLiQ interface (encoder AM22DQ) Rotatable connector PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",6412,"ST",1,"MC",16.404,1,"1FT70665WH701FG2"]
["1FT7068-5AF70-1BG0","SIMOTICS S Synchronous motor 1FT7, M0=15Nm (100K) NN=3000rpm, PN=3.42kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",4962,"ST",1,"MC",16.404,1,"1FT70685AF701BG0"]
["1FT7068-5AF70-1DG2","SIMOTICS S Synchronous motor 1FT7, M0=15Nm (100K) NN=3000rpm, PN=3.42kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",5237,"ST",1,"MC",16.404,1,"1FT70685AF701DG2"]
["1FT7068-5AF71-1NH0","SIMOTICS S Synchronous motor 1FT7, M0=15Nm (100K) NN=3000rpm, PN=3.42kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5448,"ST",1,"MC",17.702999999999999,1,"1FT70685AF711NH0"]
["1FT7068-5WF71-1NH1","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=3000rpm, PN=9.30kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6238,"ST",1,"MC",21.503,1,"1FT70685WF711NH1"]
["1FT7082-5AC71-1CH2","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=2000rpm, PN=2.39kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",6269,"ST",1,"MC",17.202999999999999,1,"1FT70825AC711CH2"]
["1FT7082-5AC71-1FH0","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=2000rpm, PN=2.39kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6167,"ST",1,"MC",17.202999999999999,1,"1FT70825AC711FH0"]
["1FT7082-5AF71-1DB3","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=3000rpm, PN=3.24kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",5513,"ST",1,"MC",17.202999999999999,1,"1FT70825AF711DB3"]
["1FT7082-5AF74-1NG1","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=3000rpm, PN=3.24kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with Pt1000 temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4037,"ST",1,"MC",14.103999999999999,1,"1FT70825AF741NG1"]
["1FT7082-5AH71-1BA2","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=4500rpm, PN=3.77kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",4487,"ST",1,"MC",14.103999999999999,1,"1FT70825AH711BA2"]
["1FT7084-1AF70-1NG1","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=3000rpm, PN=4.56kW naturally cooled; Power connector rotatable; Vibration severity A Degree of protection IP65 Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact), with KTY  temperature sensor INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACCURACY TOLERANCE N",3548,"ST",1,"MC",20.8,1,"1FT70841AF701NG1"]
["1FT7084-1AH71-1CG1","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=4500rpm, PN=4.82kW naturally cooled; Power connector rotatable; Vibration severity A Degree of protection IP65 Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACCURACY TOLERANCE N",4733,"ST",1,"MC",20.9,1,"1FT70841AH711CG1"]
["1FT7084-5AC71-1CG0","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=2000rpm, PN=3.54kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5925,"ST",1,"MC",20.904,1,"1FT70845AC711CG0"]
["1FT7084-5AC71-1MG1","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=2000rpm, PN=3.54kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",5651,"ST",1,"MC",20.904,1,"1FT70845AC711MG1"]
["1FT7084-5AF71-1CB0","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=3000rpm, PN=4.55kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6887,"ST",1,"MC",24.003,1,"1FT70845AF711CB0"]
["1FT7084-5AF71-1DG2","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=3000rpm, PN=4.55kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",5379,"ST",1,"MC",20.904,1,"1FT70845AF711DG2"]
["1FT7084-5AH71-1CB0","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=4500rpm, PN=4.82kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6887,"ST",1,"MC",24.003,1,"1FT70845AH711CB0"]
["1FT7084-5AH71-1FB0","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=4500rpm, PN=4.82kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6972,"ST",1,"MC",24.003,1,"1FT70845AH711FB0"]
["1FT7084-5SH71-1CG1","SIMOTICS S Synchronous motor 1FT7, M0=27Nm (100K) NN=4500rpm, PN=9.90kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6715,"ST",1,"MC",25.103999999999999,1,"1FT70845SH711CG1"]
["1FT7084-5WC71-1BH1","SIMOTICS S Synchronous motor 1FT7, M0=35Nm (100K) NN=2000rpm, PN=7.33kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6857,"ST",1,"MC",30.702999999999999,1,"1FT70845WC711BH1"]
["1FT7085-7SF70-1CB1","SIMOTICS S Synchronous motor 1FT7, M0=34Nm (100K) NN=3000rpm, PN=7.20kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",8716,"ST",1,"MC",37.203000000000003,1,"1FT70857SF701CB1"]
["1FT7085-7WF71-1MG1","SIMOTICS S Synchronous motor 1FT7, M0=43Nm (100K) NN=3000rpm, PN=11.90kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7377,"ST",1,"MC",32.103999999999999,1,"1FT70857WF711MG1"]
["1FT7086-5AC70-1DL4","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=2000rpm, PN=4.71kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",7633,"ST",1,"MC",30.702999999999999,1,"1FT70865AC701DL4"]
["1FT7086-5AC71-1BA2","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=2000rpm, PN=4.71kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",6336,"ST",1,"MC",27.603999999999999,1,"1FT70865AC711BA2"]
["1FT7086-5AC71-1NH1","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=2000rpm, PN=4.71kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6847,"ST",1,"MC",30.702999999999999,1,"1FT70865AC711NH1"]
["1FT7086-5AF70-1FH0","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=3000rpm, PN=5.65kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",8015,"ST",1,"MC",30.702999999999999,1,"1FT70865AF701FH0"]
["1FT7086-5AF71-1CH0","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=3000rpm, PN=5.65kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",7929,"ST",1,"MC",30.702999999999999,1,"1FT70865AF711CH0"]
["1FT7086-5AH70-1CB1","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=4500rpm, PN=4.71kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",8032,"ST",1,"MC",35.003,1,"1FT70865AH701CB1"]
["1FT7086-5SC70-1CG0","SIMOTICS S Synchronous motor 1FT7, M0=36Nm (100K) NN=2000rpm, PN=6.70kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",7654,"ST",1,"MC",36.103999999999999,1,"1FT70865SC701CG0"]
["1FT7086-5SF71-1BB4","SIMOTICS S Synchronous motor 1FT7, M0=36Nm (100K) NN=3000rpm, PN=9.10kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",8067,"ST",1,"MC",39.103000000000002,1,"1FT70865SF711BB4"]
["1FT7086-5SF71-1NB1","SIMOTICS S Synchronous motor 1FT7, M0=36Nm (100K) NN=3000rpm, PN=9.10kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7535,"ST",1,"MC",39.103000000000002,1,"1FT70865SF711NB1"]
["1FT7086-5WF71-1DH1","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=3000rpm, PN=15.40kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7985,"ST",1,"MC",37.302999999999997,1,"1FT70865WF711DH1"]
["1FT7086-5WH70-1FD4","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=4500rpm, PN=20.30kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",8181,"ST",1,"MC",34.204000000000001,1,"1FT70865WH701FD4"]
["1FT7087-7SH70-1BG0","SIMOTICS S Synchronous motor 1FT7, M0=48Nm (100K) NN=4500rpm, PN=10.80kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",7687,"ST",1,"MC",43.003999999999998,1,"1FT70877SH701BG0"]
["1FT7087-7WF71-4DA3","SIMOTICS S Synchronous motor 1FT7, M0=61Nm (100K) NN=3000rpm, PN=16.00kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTION AXIAL DE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",7939,"ST",1,"MC",41.103999999999999,1,"1FT70877WF714DA3"]
["1FT7102-5AB70-1DB0","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=1500rpm, PN=4.08kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6987,"ST",1,"MC",30.702999999999999,1,"1FT71025AB701DB0"]
["1FT7102-5AB71-1CA0","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=1500rpm, PN=4.08kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6635,"ST",1,"MC",26.204000000000001,1,"1FT71025AB711CA0"]
["1FT7102-5AC71-1DB1","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=2000rpm, PN=5.03kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7090,"ST",1,"MC",30.702999999999999,1,"1FT71025AC711DB1"]
["1FT7102-5AC71-1MD0","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=2000rpm, PN=5.03kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6429,"ST",1,"MC",26.204000000000001,1,"1FT71025AC711MD0"]
["1FT7102-5AF71-1DK3","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=3000rpm, PN=6.28kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",6238,"ST",1,"MC",26.204000000000001,1,"1FT71025AF711DK3"]
["1FT7102-5WC71-1NG0","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=2000rpm, PN=10.40kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6138,"ST",1,"MC",36.704000000000001,1,"1FT71025WC711NG0"]
["1FT7105-1AC75-1MH1","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=2000rpm, PN=7.96kW naturally cooled; Power connector rotatable; Vibration severity A Degree of protection IP65 Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact), with Pt1000  temperature sensor ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N",7005,"ST",1,"MC",48.7,1,"1FT71051AC751MH1"]
["1FT7105-5AB70-1FG0","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=1500rpm, PN=6.60kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",8356,"ST",1,"MC",44.304000000000002,1,"1FT71055AB701FG0"]
["1FT7105-5AB71-1MH0","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=1500rpm, PN=6.60kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",8979,"ST",1,"MC",48.802999999999997,1,"1FT71055AB711MH0"]
["1FT7105-5AC70-1DG1","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=2000rpm, PN=7.96kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7639,"ST",1,"MC",44.304000000000002,1,"1FT71055AC701DG1"]
["1FT7105-5AC71-1BH0","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=2000rpm, PN=7.96kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",8536,"ST",1,"MC",48.802999999999997,1,"1FT71055AC711BH0"]
["1FT7105-5AC71-1NG2","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=2000rpm, PN=7.96kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",7274,"ST",1,"MC",44.304000000000002,1,"1FT71055AC711NG2"]
["1FT7105-5AF70-1DH2","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=3000rpm, PN=8.80kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",8810,"ST",1,"MC",48.802999999999997,1,"1FT71055AF701DH2"]
["1FT7105-5AF71-1DK3","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=3000rpm, PN=8.80kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",7873,"ST",1,"MC",44.304000000000002,1,"1FT71055AF711DK3"]
["1FT7105-5AF71-1LH2","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=3000rpm, PN=8.80kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) AND M17-CONNECTOR PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",9866,"ST",1,"MC",48.802999999999997,1,"1FT71055AF711LH2"]
["1FT7105-5SF70-1CH1","SIMOTICS S Synchronous motor 1FT7, M0=65Nm (100K) NN=3000rpm, PN=15.10kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",10146,"ST",1,"MC",54.603000000000002,1,"1FT71055SF701CH1"]
["1FT7105-5SF71-1NG1","SIMOTICS S Synchronous motor 1FT7, M0=65Nm (100K) NN=3000rpm, PN=15.10kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7876,"ST",1,"MC",50.003999999999998,1,"1FT71055SF711NG1"]
["1FT7105-5SF71-7BH0","SIMOTICS S Synchronous motor 1FT7, M0=65Nm (100K) NN=3000rpm, PN=15.10kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) FOR CONNECT. OF TERMINAL BOXAND SIGNAL CONNECTOR, TERMINALBOX AXIAL NON-DRIVE END ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",9223,"ST",1,"MC",55.002000000000002,1,"1FT71055SF717BH0"]
["1FT7105-5WB71-1CH1","SIMOTICS S Synchronous motor 1FT7, M0=90Nm (100K) NN=1500rpm, PN=14.10kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",10146,"ST",1,"MC",59.402999999999999,1,"1FT71055WB711CH1"]
["1FT7105-5WF71-1NG0","SIMOTICS S Synchronous motor 1FT7, M0=90Nm (100K) NN=3000rpm, PN=24.80kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",7773,"ST",1,"MC",54.904000000000003,1,"1FT71055WF711NG0"]
["1FT7105-5WF71-5BG1","SIMOTICS S Synchronous motor 1FT7, M0=90Nm (100K) NN=3000rpm, PN=24.80kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) FOR CONNECT. OF TERMINAL BOXAND SIGNAL CONNECTOR, TERMINALBOX TRAVERSE RIGHT ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",8241,"ST",1,"MC",55.402999999999999,1,"1FT71055WF715BG1"]
["1FT7108-5AB70-1FK1","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=1500rpm, PN=9.58kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",10786,"ST",1,"MC",59.103999999999999,1,"1FT71085AB701FK1"]
["1FT7108-5AB71-1FA0","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=1500rpm, PN=9.58kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",10513,"ST",1,"MC",59.103999999999999,1,"1FT71085AB711FA0"]
["1FT7108-5AC70-1BB0","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=2000rpm, PN=10.50kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",10692,"ST",1,"MC",63.603000000000002,1,"1FT71085AC701BB0"]
["1FT7108-5AC71-1CH5","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=2000rpm, PN=10.50kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",11867,"ST",1,"MC",63.603000000000002,1,"1FT71085AC711CH5"]
["1FT7108-5AC71-1MA0","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=2000rpm, PN=10.50kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",10050,"ST",1,"MC",59.103999999999999,1,"1FT71085AC711MA0"]
["1FT7108-5AF71-1CH1","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=3000rpm, PN=6.28kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",11615,"ST",1,"MC",63.603000000000002,1,"1FT71085AF711CH1"]
["1FT7108-5SC70-1NA0","SIMOTICS S Synchronous motor 1FT7, M0=91Nm (100K) NN=2000rpm, PN=15.30kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact), with KTY  temperature sensor POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",9929,"ST",1,"MC",64.004000000000005,1,"1FT71085SC701NA0"]
["1FT7108-5SC71-5NG1","SIMOTICS S Synchronous motor 1FT7, M0=91Nm (100K) NN=2000rpm, PN=15.30kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with KTY temperature sensor FOR CONNECT. OF TERMINAL BOXAND SIGNAL CONNECTOR, TERMINALBOX TRAVERSE RIGHT INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",10032,"ST",1,"MC",64.503,1,"1FT71085SC715NG1"]
["1FT7108-5SF70-1NG0","SIMOTICS S Synchronous motor 1FT7, M0=91Nm (100K) NN=3000rpm, PN=18.80kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact), with KTY  temperature sensor POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",9929,"ST",1,"MC",64.004000000000005,1,"1FT71085SF701NG0"]
["1FT7108-5SF71-8CH1","SIMOTICS S Synchronous motor 1FT7, M0=91Nm (100K) NN=3000rpm, PN=18.80kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) FOR CONNECT. OF TERMINAL BOXAND SIGNAL CONNECTOR, TERMINALBOX AXIAL DRIVE END ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",12302,"ST",1,"MC",69.102000000000004,1,"1FT71085SF718CH1"]
["1FT7108-5WB71-1DA3","SIMOTICS S Synchronous motor 1FT7, M0=125Nm (100K) NN=1500rpm, PN=19.60kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",10546,"ST",1,"MC",68.703999999999994,1,"1FT71085WB711DA3"]
["1FT7108-5WF70-8DA3","SIMOTICS S Synchronous motor 1FT7, M0=125Nm (100K) NN=3000rpm, PN=34.20kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) FOR CONNECT. OF TERMINAL BOXAND SIGNAL CONNECTOR, TERMINALBOX AXIAL DRIVE END INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",10546,"ST",1,"MC",69.203000000000003,1,"1FT71085WF708DA3"]
["1FT7108-5WF71-8FG0","SIMOTICS S Synchronous motor 1FT7, M0=125Nm (100K) NN=3000rpm, PN=34.20kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) FOR CONNECT. OF TERMINAL BOXAND SIGNAL CONNECTOR, TERMINALBOX AXIAL DRIVE END ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",11200,"ST",1,"MC",69.203000000000003,1,"1FT71085WF718FG0"]
["1PH8083-1DF02-1BB1","SIMOTICS M Compact induction motor 1500rpm, 2.8kW 18Nm, 7.5A, 346V 1750rpm, 3.3kW 18Nm, 7.5A, 398V 2000rpm, 3.7kW 18Nm, 7.6A, 447V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5044,"ST",1,"MC",32,1,"1PH80831DF021BB1"]
["1PH8083-1DG02-0DA1","SIMOTICS M Compact induction motor 2000rpm, 3.7kW 18Nm, 11.6A, 293V 2300rpm, 4.1kW 17Nm, 11.3A, 332V 2650rpm, 4.6 kW 17Nm, 11.2A, 376V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE SR/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5328,"ST",1,"MC",32,1,"1PH80831DG020DA1"]
["1PH8083-1HF22-0BA1","SIMOTICS M Compact induction motor 1500rpm, 3.5 kW 22Nm, 8.9A, 357V 1750rpm, 4.0 kW 22Nm, 8.7A, 416V 2000rpm, 4.6 kW 22Nm, 8.7A, 457V water cooling Degree of protection IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4302,"ST",1,"MC",36,1,"1PH80831HF220BA1"]
["1PH8083-1JF20-2CA1","SIMOTICS M Compact induction motor 1500rpm, 3.5 kW 22Nm, 8.9A, 357V 1750rpm, 4.0 kW 22Nm, 8.7A, 416V 2000rpm, 4.6 kW 22Nm, 8.7A, 457V water cooling Degree of protection IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4798,"ST",1,"MC",36,1,"1PH80831JF202CA1"]
["1PH8083-1MF02-0CA1","SIMOTICS M Compact induction motor 1500rpm, 2.8kW 18Nm, 7.5A, 346V 1750rpm, 3.3kW 18Nm, 7.5A, 398V 2000rpm, 3.7kW 18Nm, 7.6A, 447V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4528,"ST",1,"MC",32,1,"1PH80831MF020CA1"]
["1PH8087-1AF22-0BC1","SIMOTICS M Compact induction motor 1500rpm, 4.6 kW 29Nm, 13.7A, 316V 1750rpm, 5.4kW 29Nm, 13.7A, 358V 2000rpm, 6.1kW 29Nm, 13.7A, 402V water cooling Degree of protection IP65 without encoder; with temperature sensor KTY 84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4051,"ST",1,"MC",44,1,"1PH80871AF220BC1"]
["1PH8087-1DG12-0DH1","SIMOTICS M Compact induction motor 2000rpm, 4.9kW 23Nm, 14.1A, 320V 2300rpm, 5.4kW 22Nm, 13.7A, 353V 2650rpm, 6.0kW 22Nm, 13.6A, 390V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE SR/A; SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY D-END SIGNAL CONNECTION LEFT",5506,"ST",1,"MC",39,1,"1PH80871DG120DH1"]
["1PH8087-1FM00-0BA1","SIMOTICS M Compact induction motor 3000rpm, 4.8 kW 15Nm, 17.3A, 284V 3300RPM, 5.2kW 15Nm, 17.1A, 303V 3600RPM 5.7kW 15Nm, 17.1A, 329V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6035,"ST",1,"MC",39,1,"1PH80871FM000BA1"]
["1PH8087-1HF22-0BC1","SIMOTICS M Compact induction motor 1500rpm, 4.6 kW 29Nm, 13.7A, 316V 1750rpm, 5.4kW 29Nm, 13.7A, 358V 2000rpm, 6.1kW 29Nm, 13.7A, 402V water cooling Degree of protection IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4476,"ST",1,"MC",44,1,"1PH80871HF220BC1"]
["1PH8087-1JM10-0BC1","SIMOTICS M Compact induction motor 3000rpm, 4.8 kW 15Nm, 17.3A, 284V 3300RPM, 5.2kW 15Nm, 17.1A, 303V 3600RPM 5.7kW 15Nm, 17.1A, 355V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4430,"ST",1,"MC",32,1,"1PH80871JM100BC1"]
["1PH8087-1UG02-0LA1","SIMOTICS M Compact induction motor 2000rpm, 4.9kW 23Nm, 14.1A, 320V 2300rpm, 5.4kW 22Nm, 13.7A, 353V 2650rpm, 6.0kW 22Nm, 13.6A, 390V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 20 BIT WITHOUT COMMUTATING POSITION (ENCODER IN20DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6030,"ST",1,"MC",39,1,"1PH80871UG020LA1"]
["1PH8101-1DF02-1CE1","SIMOTICS M Compact induction motor 1500rpm, 3.7kW 24Nm, 12.5A, 265V 2000rpm, 4.3kW 22Nm, 12.5A, 304V 2000rpm, 4.7kW 22Nm, 12.5A, 343V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5554,"ST",1,"MC",42,1,"1PH81011DF021CE1"]
["1PH8101-1HF10-0CA1","SIMOTICS M Compact induction motor 1500rpm, 3.7kW 24Nm, 12.5A, 265V 1750rpm, 4.3kW 23Nm, 12.5A, 304V 2000rpm, 4.7kW 22Nm, 12.5A, 343V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4266,"ST",1,"MC",42,1,"1PH81011HF100CA1"]
["1PH8101-1JF13-0BC1","SIMOTICS M Compact induction motor 1500rpm, 3.7kW 24Nm, 12.5A, 265V 1750rpm, 4.3kW 23Nm, 12.5A, 304V 2000rpm, 4.7kW 22Nm, 12.5A, 343V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4971,"ST",1,"MC",42,1,"1PH81011JF130BC1"]
["1PH8101-1JF23-0BC1","SIMOTICS M Compact induction motor 1500rpm, 5 kW 32Nm, 12.8A, 357V 1750rpm, 5.8kW 32Nm, 12.8A, 400 V 2000rpm, 6.6kW 32Nm, 12.5A, 450 V water cooling Degree of protection IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5390,"ST",1,"MC",51,1,"1PH81011JF230BC1"]
["1PH8103-1AF22-2CB1","SIMOTICS M Compact induction motor 1500rpm, 7.1kW 45Nm, 19.7A, 317V 1750rpm, 8.2kW 45Nm, 19.7A, 364V 2000rpm, 9.4kW 45Nm, 19.7A, 411V water cooling Degree of protection IP65 without encoder; with temperature sensor KTY 84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4608,"ST",1,"MC",60,1,"1PH81031AF222CB1"]
["1PH8103-1AM23-2BA1","SIMOTICS M Compact induction motor 3000rpm, 10.6kW 34Nm, 30 A, 309V 3300RPM, 11.7kW 34Nm, 30 A, 340V 3600RPM 12.7kW 34Nm, 29.7A, 368V water cooling Degree of protection IP65 without encoder; with temperature sensor KTY 84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4655,"ST",1,"MC",60,1,"1PH81031AM232BA1"]
["1PH8103-1DG00-2CA1","SIMOTICS M Compact induction motor 2000rpm, 7.0 kW 31Nm, 17A, 345V 2300rpm, 7.5kW 33Nm, 17.5A, 400 V 2650rpm, 8.0kW 29Nm, 16A, 434V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5460,"ST",1,"MC",51,1,"1PH81031DG002CA1"]
["1PH8103-1DG03-0CE1","SIMOTICS M Compact induction motor 2000rpm, 7.0 kW 31Nm, 17A, 345V 2300rpm, 7.5kW 33Nm, 17.5A, 400 V 2650rpm, 8.0kW 29Nm, 16A, 434V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5924,"ST",1,"MC",51,1,"1PH81031DG030CE1"]
["1PH8103-1DM22-1CC1","SIMOTICS M Compact induction motor 3000rpm, 10.6kW 34Nm, 30 A, 309V 3300RPM, 11.7kW 34Nm, 30 A, 340V 3600RPM 12.7kW 34Nm, 29.7A, 368V water cooling Degree of protection IP65 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",6112,"ST",1,"MC",60,1,"1PH81031DM221CC1"]
["1PH8103-1HF10-0BC1","SIMOTICS M Compact induction motor 1500rpm, 5.5 kW 35Nm, 13.1A, 368V 1750rpm, 6.3kW 34Nm, 13.5A, 412V 2000rpm, 7 kW 33Nm, 12.7A, 460 V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4171,"ST",1,"MC",51,1,"1PH81031HF100BC1"]
["1PH8103-1JD12-0BA1","SIMOTICS M Compact induction motor 1000rpm, 3.7kW 35Nm, 10A, 333V 1150rpm, 4.3kW 36Nm, 10A, 380 V 1350rpm, 4.7kW 33Nm, 9.7A, 423V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4830,"ST",1,"MC",51,1,"1PH81031JD120BA1"]
["1PH8103-1JF03-1BA1","SIMOTICS M Compact induction motor 1500rpm, 5.5 kW 35Nm, 13.1A, 342V 1750rpm, 6.3kW 34Nm, 13.5A, 412V 2000rpm, 7.0 kW 33Nm, 12.7A, 460 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5086,"ST",1,"MC",51,1,"1PH81031JF031BA1"]
["1PH8103-1JF22-0CC1","SIMOTICS M Compact induction motor 1500rpm, 7.1kW 45Nm, 19.7A, 317V 1750rpm, 8.2kW 45Nm, 19.7A, 364V 2000rpm, 9.4kW 45Nm, 19.7A, 411V water cooling Degree of protection IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5483,"ST",1,"MC",60,1,"1PH81031JF220CC1"]
["1PH8105-1AF12-2CA1","SIMOTICS M Compact induction motor 1500rpm, 7kW, 45Nm, 17.5A, 348V 1750rpm, 8kW, 44Nm, 17.5A, 400 V 2000rpm, 9kW, 43Nm, 17A, 453V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 without encoder; with temperature sensor KTY 84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4369,"ST",1,"MC",65,1,"1PH81051AF122CA1"]
["1PH8105-1AF23-0CB1","SIMOTICS M Compact induction motor 1500rpm, 11 kW 70 Nm, 28.5A, 340V 1750rpm, 12.5kW 68Nm, 28.5A, 380 V 2000rpm, 14kW 67Nm, 27.5A, 426V water cooling Degree of protection IP65 without encoder; with temperature sensor KTY 84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5189,"ST",1,"MC",74,1,"1PH81051AF230CB1"]
["1PH8105-1DF23-0CA1","SIMOTICS M Compact induction motor 1500rpm, 11 kW 70 Nm, 28.5A, 340V 1750rpm, 12.5kW 68Nm, 28.5A, 380 V 2000rpm, 14kW 67Nm, 27.5A, 426V water cooling Degree of protection IP65 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6693,"ST",1,"MC",74,1,"1PH81051DF230CA1"]
["1PH8105-1FF23-0BA1","SIMOTICS M Compact induction motor 1500rpm, 11 kW 70 Nm, 28.5A, 340V 1750rpm, 12.5kW 68Nm, 28.5A, 380 V 2000rpm, 14kW 67Nm, 27.5A, 426V water cooling Degree of protection IP65 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7460,"ST",1,"MC",74,1,"1PH81051FF230BA1"]
["1PH8105-1JF02-2BA1","SIMOTICS M Compact induction motor 1500rpm, 7.0 kW 45Nm, 17.5A, 348V 1750rpm, 8.0kW 44Nm, 17.5A, 400 V 2000rpm, 9.0kW 43Nm, 17.0A, 453V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5035,"ST",1,"MC",65,1,"1PH81051JF022BA1"]
["1PH8105-1JF12-2BC1","SIMOTICS M Compact induction motor 1500rpm, 7kW, 45Nm, 17.5A, 348V 1750rpm, 8kW, 44Nm, 17.5A, 400 V 2000rpm, 9kW, 43Nm, 17A, 453V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5035,"ST",1,"MC",65,1,"1PH81051JF122BC1"]
["1PH8105-3FF03-2AA1","SIMOTICS M Compact induction motor 1500rpm, 7.0 kW 45Nm, 17.5A, 348V 1750rpm, 8.0kW 44Nm, 17.5A, 400 V 2000rpm, 9.0kW 43Nm, 17.0A, 453V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD VIBRATION SEVERITY GRADE A; SHAFT A.FLANGE ACCURACY GR.N TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6522,"ST",1,"MC",65,1,"1PH81053FF032AA1"]
["1PH8107-1AD12-2BC1","SIMOTICS M Compact induction motor 1000rpm, 6.3kW 60Nm, 17.5A, 307V 1150rpm, 7.2kW 60Nm, 17.5A, 348V 1350rpm, 8kW 57Nm, 17A, 400 V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 without encoder; with temperature sensor KTY 84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4311,"ST",1,"MC",73,1,"1PH81071AD122BC1"]
["1PH8107-1AG02-0BA1","SIMOTICS M Compact induction motor 2000rpm, 10.5kW 50Nm, 26 A, 355V 2300rpm, 12kW 50Nm, 26 A, 406V 2650rpm, 13kW 47Nm, 24A, 460 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 without encoder; with temperature sensor KTY 84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4311,"ST",1,"MC",73,1,"1PH81071AG020BA1"]
["1PH8107-1CS02-3LA1","SIMOTICS M Compact induction motor Y2000RPM, 11 kW 53Nm, 26.7A, 368V D5000RPM, 11 kW 21Nm, 28A, 410V Y1500RPM, 8.5kW 54Nm, 27A, 275V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER SIN/COS 1VPP 256 S/R WITHOUT ND-END AT TERMINAL BOX (ENCODER IN256S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN HOLLOW-SHAFT BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8735,"ST",1,"MC",75.5,1,"1PH81071CS023LA1"]
["1PH8107-1DD10-2BA1","SIMOTICS M Compact induction motor 1000rpm, 6.3kW 60Nm, 17.5A, 307V 1150rpm, 7.2kW 60Nm, 17.5A, 348V 1350rpm, 8kW 57Nm, 17A, 400 V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5607,"ST",1,"MC",73,1,"1PH81071DD102BA1"]
["1PH8107-1DF02-0BE1","SIMOTICS M Compact induction motor 1500rpm, 9.0kW 57Nm, 23.5A, 330V 1750rpm, 10.0kW 55Nm, 22A, 380 V 2000rpm, 11 kW 53Nm, 21.5A, 428V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5816,"ST",1,"MC",73,1,"1PH81071DF020BE1"]
["1PH8107-1DF23-1CC1","SIMOTICS M Compact induction motor 1500rpm, 14kW 89Nm, 43.4A, 277V 1750rpm, 15.5kW 85Nm, 42A, 314V 2000rpm, 18kW 86Nm, 42.6A, 363V water cooling Degree of protection IP65 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",7065,"ST",1,"MC",83,1,"1PH81071DF231CC1"]
["1PH8107-1DG02-0CF1","SIMOTICS M Compact induction motor 2000rpm, 10.5kW 50Nm, 26 A, 355V 2300rpm, 12kW 50Nm, 26 A, 406V 2650rpm, 13kW 47Nm, 24A, 460 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",6025,"ST",1,"MC",73,1,"1PH81071DG020CF1"]
["1PH8107-1DG12-2BB1","SIMOTICS M Compact induction motor 2000rpm, 10.5kW 50Nm, 26 A, 355V 2300rpm, 12.5kW 50Nm, 26 A, 406V 2650rpm, 13kW 47Nm, 24A, 460 V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5816,"ST",1,"MC",73,1,"1PH81071DG122BB1"]
["1PH8107-1FD03-1BA1","SIMOTICS M Compact induction motor 1000rpm, 6.3kW 60Nm, 17.5A, 307V 1150rpm, 7.2kW 60Nm, 17.5A, 348V 1350rpm, 8.0kW 57Nm, 17A, 400 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7047,"ST",1,"MC",73,1,"1PH81071FD031BA1"]
["1PH8107-1FF13-1BC1","SIMOTICS M Compact induction motor 1500rpm, 9kW 57Nm, 23.5A, 330V 1750rpm, 10 kW 55Nm, 22A, 380 V 2000rpm, 11 kW 53Nm, 21.5A, 428V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",7047,"ST",1,"MC",73,1,"1PH81071FF131BC1"]
["1PH8107-1HD13-1BA1","SIMOTICS M Compact induction motor 1000rpm, 6.3kW 60Nm, 17.5A, 307V 1150rpm, 7.2kW 60Nm, 17.5A, 348V 1350rpm, 8kW 57Nm, 17A, 400 V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4992,"ST",1,"MC",73,1,"1PH81071HD131BA1"]
["1PH8107-1HF10-0BC1","SIMOTICS M Compact induction motor 1500rpm, 9kW 57Nm, 23.5A, 330V 1750rpm, 10 kW 55Nm, 22A, 380 V 2000rpm, 11 kW 53Nm, 21.5A, 428V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4527,"ST",1,"MC",73,1,"1PH81071HF100BC1"]
["1PH8107-1HG10-0BB1","SIMOTICS M Compact induction motor 2000rpm, 10.5kW 50Nm, 26 A, 355V 2300rpm, 12.5kW 50Nm, 26 A, 406V 2650rpm, 13kW 47Nm, 24A, 460 V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4527,"ST",1,"MC",73,1,"1PH81071HG100BB1"]
["1PH8107-1JD12-0CC1","SIMOTICS M Compact induction motor 1000rpm, 6.3kW 60Nm, 17.5A, 307V 1150rpm, 7.2kW 60Nm, 17.5A, 348V 1350rpm, 8kW 57Nm, 17A, 400 V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5395,"ST",1,"MC",73,1,"1PH81071JD120CC1"]
["1PH8107-1JF23-2BC1","SIMOTICS M Compact induction motor 1500rpm, 14kW 89Nm, 43.4A, 277V 1750rpm, 15.5kW 85Nm, 42A, 314V 2000rpm, 18kW 86Nm, 42.6A, 363V water cooling Degree of protection IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",6226,"ST",1,"MC",83,1,"1PH81071JF232BC1"]
["1PH8107-1MF02-2HA2","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 9,0KW,57NM,23,5A, 330V 1750RPM, 10,0KW,55NM, 22A, 380V 2000RPM, 11KW,53NM, 21,5A, 428V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERATURE SENSOR PT1000 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4976,"ST",1,"MC",73,1,"1PH81071MF022HA2"]
["1PH8107-1SM03-1LA1","SIMOTICS M Compact induction motor 3000rpm, 12kW 38Nm, 38A, 294V 3300RPM, 13kW 38Nm, 38A, 326V 3600RPM 14kW 37Nm, 37.5A, 355V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 19 BIT WITH COMMUTATING POSITION (ENCODER IN19DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8061,"ST",1,"MC",73,1,"1PH81071SM031LA1"]
["1PH8107-1UG03-2LA1","SIMOTICS M Compact induction motor 2000rpm, 10.5kW 50Nm, 26 A, 355V 2300rpm, 12kW 50Nm, 26 A, 406V 2650rpm, 13kW 47Nm, 24A, 460 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 20 BIT WITHOUT COMMUTATING POSITION (ENCODER IN20DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6842,"ST",1,"MC",73,1,"1PH81071UG032LA1"]
["1PH8131-1DF00-0LE1","SIMOTICS M Compact induction motor 1500rpm, 11kW, 70 Nm, 24A, 360V 1750rpm, 13kW, 71Nm, 24A, 416V 2000rpm, 15 kW, 72Nm, 24A, 460 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6363,"ST",1,"MC",89,1,"1PH81311DF000LE1"]
["1PH8131-1DF10-0CB1","SIMOTICS M Compact induction motor 1500rpm, 11kW, 70 Nm, 24A, 360V 1750rpm, 13kW, 71Nm, 24A, 416V 2000rpm, 15 kW, 72Nm, 24A, 460 V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5986,"ST",1,"MC",89,1,"1PH81311DF100CB1"]
["1PH8131-1DF10-2BA1","SIMOTICS M Compact induction motor 1500rpm, 11kW, 70 Nm, 24A, 360V 1750rpm, 13kW, 71Nm, 24A, 416V 2000rpm, 15 kW, 72Nm, 24A, 460 V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5777,"ST",1,"MC",89,1,"1PH81311DF102BA1"]
["1PH8131-1HF00-1GB1","SIMOTICS M Compact induction motor 1500rpm, 11kW, 70 Nm, 24A, 360V 1750rpm, 13kW, 71Nm, 24A, 416V 2000rpm, 15 kW, 72Nm, 24A, 460 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4392,"ST",1,"MC",89,1,"1PH81311HF001GB1"]
["1PH8131-1JF00-2GA1","SIMOTICS M Compact induction motor 1500rpm, 11kW, 70 Nm, 24A, 360V 1750rpm, 13kW, 71Nm, 24A, 416V 2000rpm, 15 kW, 72Nm, 24A, 460 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4842,"ST",1,"MC",89,1,"1PH81311JF002GA1"]
["1PH8131-1JF20-2BC1","SIMOTICS M Compact induction motor 1500rpm, 15 kW 96Nm, 30 A, 380 V 1750rpm, 17kW 93Nm, 30 A, 425V 2000rpm, 18.5 kW 88Nm, 30 A, 460 V water cooling Degree of protection IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5971,"ST",1,"MC",105,1,"1PH81311JF202BC1"]
["1PH8131-1MF20-2CE1","SIMOTICS M Compact induction motor 1500rpm, 15 kW 96Nm, 30 A, 380 V 1750rpm, 17kW 93Nm, 30 A, 425V 2000rpm, 18.5 kW 88Nm, 30 A, 460 V water cooling Degree of protection IP65 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6085,"ST",1,"MC",105,1,"1PH81311MF202CE1"]
["1PH8131-2DF02-1CA1","SIMOTICS M Compact synchronous motor 1500rpm, 15.7kW 100 Nm, 29A, 388V 1750rpm, 18kW 98Nm, 29A, 415 V 2000rpm, 19.9kW 95Nm, 29A, 449V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",11967,"ST",1,"MC",85,1,"1PH81312DF021CA1"]
["1PH8131-2FF02-0BA1","SIMOTICS M Compact synchronous motor 1500rpm, 15.7kW 100 Nm, 29A, 388V 1750rpm, 18kW 98Nm, 29A, 415 V 2000rpm, 19.9kW 95Nm, 29A, 449V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",12734,"ST",1,"MC",85,1,"1PH81312FF020BA1"]
["1PH8133-1AF00-1BB1","SIMOTICS M Compact induction motor 1500rpm, 15 kW 96Nm, 34A, 342V 1750rpm, 17.5kW 96Nm, 34A, 392V 2000rpm, 20 kW 96Nm, 34A, 445V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 without encoder; with temperature sensor KTY 84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4407,"ST",1,"MC",106,1,"1PH81331AF001BB1"]
["1PH8133-1AF20-0BC1","SIMOTICS M Compact induction motor 1500rpm, 17kW, 108Nm, 38A, 345V 1750rpm, 19.5kW, 106Nm, 38A, 40 2000rpm, 22.5kW, 107Nm, 38A, 45 water cooling Degree of protection IP65 without encoder; with temperature sensor KTY 84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5270,"ST",1,"MC",123,1,"1PH81331AF200BC1"]
["1PH8133-1DD00-2QG1","SIMOTICS M Compact induction motor 1000rpm, 12kW 115Nm, 30 A, 319V 1150rpm, 13.5kW 112Nm, 29A, 361V 1350rpm, 15 kW 106Nm, 28A, 417V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: ADVANCED LIFETIME VIBRATION SEVERITY S/A SHAFT A. FLANGE ACCURACY GR. R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",6372,"ST",1,"MC",106,1,"1PH81331DD002QG1"]
["1PH8133-1DD13-2BA1","SIMOTICS M Compact induction motor 1000rpm, 12kW 115Nm, 30 A, 319V 1150rpm, 13.5kW 112Nm, 29A, 361V 1350rpm, 15 kW 106Nm, 28A, 417V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6491,"ST",1,"MC",106,1,"1PH81331DD132BA1"]
["1PH8133-1DF02-2GA1","SIMOTICS M Compact induction motor 1500rpm, 15 kW 96Nm, 34A, 342V 1750rpm, 17.5kW 96Nm, 34A, 392V 2000rpm, 20 kW 96Nm, 34A, 445V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5861,"ST",1,"MC",106,1,"1PH81331DF022GA1"]
["1PH8133-1DF10-1BE1","SIMOTICS M Compact induction motor 1500rpm, 15 kW 96Nm, 34A, 342V 1750rpm, 17.5kW 96Nm, 34A, 392V 2000rpm, 20 kW 96Nm, 34A, 445V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5911,"ST",1,"MC",106,1,"1PH81331DF101BE1"]
["1PH8133-1DG02-1LG1","SIMOTICS M Compact induction motor 2000rpm, 20 kW 96Nm, 45 A, 350 V 2300rpm, 22.5kW 93Nm, 44A, 400 V 2650rpm, 24 kW 86Nm, 41A, 456V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",6752,"ST",1,"MC",106,1,"1PH81331DG021LG1"]
["1PH8133-1DG12-1GB1","SIMOTICS M Compact induction motor 2000rpm, 20 kW 96Nm, 45 A, 350 V 2300rpm, 22.5kW 93Nm, 44A, 400 V 2650rpm, 24 kW 86Nm, 41A, 456V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5861,"ST",1,"MC",106,1,"1PH81331DG121GB1"]
["1PH8133-1FF02-0CE1","SIMOTICS M Compact induction motor 1500rpm, 15 kW 96Nm, 34A, 342V 1750rpm, 17.5kW 96Nm, 34A, 392V 2000rpm, 20 kW 96Nm, 34A, 445V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7351,"ST",1,"MC",106,1,"1PH81331FF020CE1"]
["1PH8133-1HD10-0BC1","SIMOTICS M Compact induction motor 1000rpm, 12kW 115Nm, 30 A, 319V 1150rpm, 13.5kW 112Nm, 29A, 361V 1350rpm, 15 kW 106Nm, 28A, 417V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4831,"ST",1,"MC",106,1,"1PH81331HD100BC1"]
["1PH8133-1HF12-2BE1","SIMOTICS M Compact induction motor 1500rpm, 15 kW 96Nm, 34A, 342V 1750rpm, 17.5kW 96Nm, 34A, 392V 2000rpm, 20 kW 96Nm, 34A, 445V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5087,"ST",1,"MC",106,1,"1PH81331HF122BE1"]
["1PH8133-1HF20-2CA1","SIMOTICS M Compact induction motor 1500rpm, 17kW, 108Nm, 38A, 345V 1750rpm, 19.5kW, 106Nm, 38A, 40 2000rpm, 22.5kW, 107Nm, 38A, 45 water cooling Degree of protection IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5904,"ST",1,"MC",123,1,"1PH81331HF202CA1"]
["1PH8133-1HG03-2BB2","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 20KW, 96NM, 45A, 350V 2300RPM,22,5KW, 93NM, 44A, 400V 2650RPM, 24KW, 86NM, 41A, 456V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERATURE SENSOR PT1000 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5400,"ST",1,"MC",106,1,"1PH81331HG032BB2"]
["1PH8133-1JF22-2CB1","SIMOTICS M Compact induction motor 1500rpm, 17kW, 108Nm, 38A, 345V 1750rpm, 19.5kW, 106Nm, 38A, 40 2000rpm, 22.5kW, 107Nm, 38A, 45 water cooling Degree of protection IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",6610,"ST",1,"MC",123,1,"1PH81331JF222CB1"]
["1PH8133-1MD00-0DA1","SIMOTICS M Compact induction motor 1000rpm, 12kW 115Nm, 30 A, 319V 1150rpm, 13.5kW 112Nm, 29A, 361V 1350rpm, 15 kW 106Nm, 28A, 417V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: SR/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5471,"ST",1,"MC",106,1,"1PH81331MD000DA1"]
["1PH8133-1SF00-1LA1","SIMOTICS M Compact induction motor 1500rpm, 15 kW 96Nm, 34A, 342V 1750rpm, 17.5kW 96Nm, 34A, 392V 2000rpm, 20 kW 96Nm, 34A, 445V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 19 BIT WITHOUT COMMUTATION POSITION (ENCODER IN19DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7937,"ST",1,"MC",106,1,"1PH81331SF001LA1"]
["1PH8133-2DF02-1BE1","SIMOTICS M Compact synchronous motor 1500rpm, 19.9kW 127Nm, 44A, 316V 1750rpm, 23.1kW 126Nm, 43A, 366V 2000rpm, 26.2kW 125Nm, 43A, 415 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",12281,"ST",1,"MC",103,1,"1PH81332DF021BE1"]
["1PH8133-2FF00-0CA1","SIMOTICS M Compact synchronous motor 1500rpm, 19.9kW 127Nm, 44A, 316V 1750rpm, 23.1kW 126Nm, 43A, 366V 2000rpm, 26.2kW 125Nm, 43A, 415 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",13210,"ST",1,"MC",103,1,"1PH81332FF000CA1"]
["1PH8135-1AB00-2BA1","SIMOTICS M Compact induction motor 400rpm, 6.4kW, 153Nm, 18A, 320V 500rpm, 8kW, 153Nm, 18A, 380 V 600rpm, 9.6kW, 153Nm, 18A, 443V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 without encoder; with temperature sensor KTY 84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4854,"ST",1,"MC",125,1,"1PH81351AB002BA1"]
["1PH8135-1CF22-3LA1","SIMOTICS M Compact induction motor 1500rpm, 22kW, 140 Nm, 51A, 342V 1750rpm, 25.5kW, 139Nm, 51A, 39 2000rpm, 29kW, 138Nm, 52A, 448V water cooling Degree of protection IP65 INCREMENTAL ENCODER SIN/COS 1VPP 256 S/R WITHOUT ND-END AT TERMINAL BOX (ENCODER IN256S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN HOLLOW-SHAFT BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",10672,"ST",1,"MC",143.5,1,"1PH81351CF223LA1"]
["1PH8135-1DF00-2QA1","SIMOTICS M Compact induction motor 1500rpm, 18.5 kW 118Nm, 43A, 330V 1750rpm, 21.5kW 117Nm, 43A, 383V 2000rpm, 24 kW 115Nm, 43A, 434V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: ADVANCED LIFETIME VIBRATION SEVERITY S/A SHAFT A. FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6820,"ST",1,"MC",125,1,"1PH81351DF002QA1"]
["1PH8135-1DF23-0DH1","SIMOTICS M Compact induction motor 1500rpm, 22kW, 140 Nm, 51A, 342V 1750rpm, 25.5kW, 139Nm, 51A, 39 2000rpm, 29kW, 138Nm, 52A, 448V water cooling Degree of protection IP65 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: SR/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE D-END SIGNAL CONNECTION LEFT",8243,"ST",1,"MC",141,1,"1PH81351DF230DH1"]
["1PH8135-1FF02-0GB1","SIMOTICS M Compact induction motor 1500rpm, 18.5 kW 118Nm, 43A, 330V 1750rpm, 21.5kW 117Nm, 43A, 383V 2000rpm, 24 kW 115Nm, 43A, 434V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",7284,"ST",1,"MC",125,1,"1PH81351FF020GB1"]
["1PH8135-1HF20-2CB1","SIMOTICS M Compact induction motor 1500rpm, 22kW, 140 Nm, 51A, 342V 1750rpm, 25.5kW, 139Nm, 51A, 39 2000rpm, 29kW, 138Nm, 52A, 448V water cooling Degree of protection IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",6508,"ST",1,"MC",141,1,"1PH81351HF202CB1"]
["1PH8135-1JF13-0BB1","SIMOTICS M Compact induction motor 1500rpm, 18.5 kW 118Nm, 43A, 330V 1750rpm, 21.5kW 117Nm, 43A, 383V 2000rpm, 24 kW 115Nm, 43A, 434V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",6310,"ST",1,"MC",125,1,"1PH81351JF130BB1"]
["1PH8135-1MS00-0BA1","SIMOTICS M Compact induction motor 2000rpm, 24.5kW, 117Nm, 51A, 372V; 5000rpm, 18.5kW, 47Nm, 52A, 425V; 1500rpm, 18.5kW, 118Nm, 51A, 283V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5634,"ST",1,"MC",125,1,"1PH81351MS000BA1"]
["1PH8135-1SS02-3LA1","SIMOTICS M Compact induction motor 2000rpm, 24.5kW, 117Nm, 51A, 372V; 5000rpm, 18.5kW, 47Nm, 52A, 425V; 1500rpm, 18.5kW, 118Nm, 51A, 283V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 19 BIT WITHOUT COMMUTATION POSITION (ENCODER IN19DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN HOLLOW-SHAFT BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",10348,"ST",1,"MC",127.5,1,"1PH81351SS023LA1"]
["1PH8135-2DF02-2CA1","SIMOTICS M Compact synchronous motor 1500rpm, 23.7kW 151Nm, 43A, 383V 1750rpm, 27.2kW 149Nm, 42A, 415 V 2000rpm, 30.2kW 144Nm, 42A, 449V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",13012,"ST",1,"MC",120,1,"1PH81352DF022CA1"]
["1PH8135-2MG22-2BH1","SIMOTICS M Compact synchronous motor 2000rpm, 39kW 186Nm, 81A, 346V 2300rpm, 44.3kW 184Nm, 80 A, 395V 2300rpm, 44.3kW 184Nm, 80 A, 395V water cooling Degree of protection IP65 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE D-END SIGNAL CONNECTION LEFT",11972,"ST",1,"MC",138,1,"1PH81352MG222BH1"]
["1PH8137-1AF00-1GC1","SIMOTICS M Compact induction motor 1500rpm, 22kW, 140 Nm, 56A, 308V 1750rpm, 25kW, 136Nm, 56A, 352V 2000rpm, 28kW, 134Nm, 55A, 401V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 without encoder; with temperature sensor KTY 84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4845,"ST",1,"MC",141,1,"1PH81371AF001GC1"]
["1PH8137-1CD02-3MA1","SIMOTICS M Compact induction motor 1000rpm, 17kW 162Nm, 43A, 307V 1150rpm, 19.5kW 162Nm, 43A, 350 V 1350rpm, 22 kW 156Nm, 42A, 404V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER SIN/COS 1VPP 256 S/R WITHOUT ND-END AT TERMINAL BOX (ENCODER IN256S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN HOLLOW-SHAFT BEARING: HIGH PERFORMANCE VIBRATION SEVERITY GRADE SPECIAL/B SHAFT AND FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",10669,"ST",1,"MC",143.5,1,"1PH81371CD023MA1"]
["1PH8137-1DB02-1HA1","SIMOTICS M Compact induction motor 400rpm 6.9kW 165Nm 18A 323V 500rpm 8.6kW 165Nm 18A 391V 600rpm 10.3kW 165Nm 18A 458V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6813,"ST",1,"MC",141,1,"1PH81371DB021HA1"]
["1PH8137-1DD10-0CA1","SIMOTICS M Compact induction motor 1000rpm, 17kW 162Nm, 43A, 307V 1150rpm, 19.5kW 162Nm, 43A, 350 V 1350rpm, 22 kW 156Nm, 42A, 404V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6863,"ST",1,"MC",141,1,"1PH81371DD100CA1"]
["1PH8137-1DF00-1CA1","SIMOTICS M Compact induction motor 1500rpm, 22kW, 140 Nm, 56A, 308V 1750rpm, 25kW, 136Nm, 56A, 352V 2000rpm, 28kW, 134Nm, 55A, 401V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6863,"ST",1,"MC",141,1,"1PH81371DF001CA1"]
["1PH8137-1DF13-2BC1","SIMOTICS M Compact induction motor 1500rpm, 22kW, 140 Nm, 56A, 308V 1750rpm, 25kW, 136Nm, 56A, 353V 2000rpm, 28kW, 134Nm, 55A, 401V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",7235,"ST",1,"MC",141,1,"1PH81371DF132BC1"]
["1PH8137-1DG02-0BE1","SIMOTICS M Compact induction motor 2000rpm, 28kW, 134Nm, 60A, 350 V 2300rpm, 29kW, 120Nm, 56A, 400 V 2650rpm, 30 kW, 108Nm, 52A, 460 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6910,"ST",1,"MC",141,1,"1PH81371DG020BE1"]
["1PH8137-1EF12-1BA1","SIMOTICS M Compact induction motor 1500rpm, 22kW, 140 Nm, 56A, 308V 1750rpm, 25kW, 136Nm, 56A, 353V 2000rpm, 28kW, 134Nm, 55A, 401V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER AM2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7180,"ST",1,"MC",141,1,"1PH81371EF121BA1"]
["1PH8137-1FD10-2FA1","SIMOTICS M Compact induction motor 1000rpm, 17kW 162Nm, 43A, 307V 1150rpm, 19.5kW 162Nm, 43A, 350 V 1350rpm, 22 kW 156Nm, 42A, 404V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: INCREASED RADIAL FORCES, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7770,"ST",1,"MC",141,1,"1PH81371FD102FA1"]
["1PH8137-1HD13-2CB1","SIMOTICS M Compact induction motor 1000rpm, 17kW 162Nm, 43A, 307V 1150rpm, 19.5kW 162Nm, 43A, 350 V 1350rpm, 22 kW 156Nm, 42A, 404V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",6364,"ST",1,"MC",141,1,"1PH81371HD132CB1"]
["1PH8137-1HF02-0DC1","SIMOTICS M Compact induction motor 1500rpm, 22kW, 140 Nm, 56A, 308V 1750rpm, 25kW, 136Nm, 56A, 352V 2000rpm, 28kW, 134Nm, 55A, 401V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: SR/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",6114,"ST",1,"MC",141,1,"1PH81371HF020DC1"]
["1PH8137-1HG02-2CA1","SIMOTICS M Compact induction motor 2000rpm, 28kW, 134Nm, 60A, 350 V 2300rpm, 29kW, 120Nm, 56A, 400 V 2650rpm, 30 kW, 108Nm, 52A, 460 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6039,"ST",1,"MC",141,1,"1PH81371HG022CA1"]
["1PH8137-1JD12-0BC1","SIMOTICS M Compact induction motor 1000rpm, 17kW 162Nm, 43A, 307V 1150rpm, 19.5kW 162Nm, 43A, 350 V 1350rpm, 22 kW 156Nm, 42A, 404V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",6280,"ST",1,"MC",141,1,"1PH81371JD120BC1"]
["1PH8137-1JF23-0CC1","SIMOTICS M Compact induction motor 1500rpm, 27kW 172Nm, 67A, 315V 1750rpm, 31.5kW 172Nm, 67A, 365V 2000rpm, 36 kW 172Nm, 67A, 415 V water cooling Degree of protection IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",8108,"ST",1,"MC",157,1,"1PH81371JF230CC1"]
["1PH8137-1MD12-2BB1","SIMOTICS M Compact induction motor 1000rpm, 17kW 162Nm, 43A, 307V 1150rpm, 19.5kW 162Nm, 43A, 350 V 1350rpm, 22 kW 156Nm, 42A, 404V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",6185,"ST",1,"MC",141,1,"1PH81371MD122BB1"]
["1PH8137-1SF20-0LH1","SIMOTICS M Compact induction motor 1500rpm, 27kW 172Nm, 67A, 315V 1750rpm, 31.5kW 172Nm, 67A, 365V 2000rpm, 36 kW 172Nm, 67A, 415 V water cooling Degree of protection IP65 INCREMENTAL ENCODER 19 BIT WITHOUT COMMUTATION POSITION (ENCODER IN19DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE D-END SIGNAL CONNECTION LEFT",9973,"ST",1,"MC",157,1,"1PH81371SF200LH1"]
["1PH8137-1UF02-0LA1","SIMOTICS M Compact induction motor 1500rpm, 22kW, 140 Nm, 56A, 308V 1750rpm, 25kW, 136Nm, 56A, 352V 2000rpm, 28kW, 134Nm, 55A, 401V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 20 BIT WITHOUT COMMUTATION POSITION (ENCODER IN20DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7717,"ST",1,"MC",141,1,"1PH81371UF020LA1"]
["1PH8137-1US00-2LA1","SIMOTICS M Compact induction motor 2000rpm, 29kW 138Nm, 56A, 398V 5000rpm, 27.5kW 53Nm, 56A, 425V 1500rpm, 22 kW 140 Nm, 56A, 308V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 20 BIT WITHOUT COMMUTATION POSITION (ENCODER IN20DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7461,"ST",1,"MC",141,1,"1PH81371US002LA1"]
["1PH8137-2DM12-0QC1","SIMOTICS M Compact synchronous motor 3000rpm, 57.5kW 183Nm, 104A, 370 3300RPM, 62.2kW 180Nm, 102A, 405 3600RPM 66.7kW 177Nm, 100 A, 440 forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: ADVANCED LIFETIME VIBRATION SEVERITY S/A SHAFT A. FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",14378,"ST",1,"MC",136,1,"1PH81372DM120QC1"]
["1PH8137-2FL02-2BA1","SIMOTICS M Compact synchronous motor 2500rpm, 48.4kW 185Nm, 83A, 371V 2800rpm, 53.4kW 182Nm, 82A, 415 V 3000rpm, 56.9kW 181Nm, 81A, 449V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",14892,"ST",1,"MC",136,1,"1PH81372FL022BA1"]
["1PH8138-1FF20-1DC1","SIMOTICS M Compact induction motor 1500rpm, 30 kW, 191Nm, 80 A, 289V 1750rpm, 33 kW, 180Nm, 77A, 332V 2000rpm, 37kW, 177Nm, 76A, 380 V water cooling Degree of protection IP65 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: SR/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",9556,"ST",1,"MC",160,1,"1PH81381FF201DC1"]
["1PH8138-1HF23-0CB1","SIMOTICS M Compact induction motor 1500rpm, 30 kW, 191Nm, 80 A, 289V 1750rpm, 33 kW, 180Nm, 77A, 332V 2000rpm, 37kW, 177Nm, 76A, 380 V water cooling Degree of protection IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",8006,"ST",1,"MC",160,1,"1PH81381HF230CB1"]
["1PH8163-1AB12-0BC1","SIMOTICS M Compact induction motor 400rpm, 9.5kW 227Nm, 30 A, 260V 500rpm, 12kW 229Nm, 30 A, 325V 600rpm, 14.5kW 231Nm, 30 A, 370V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",6854,"ST",1,"MC",196,1,"1PH81631AB120BC1"]
["1PH8163-1AD10-0BA1","SIMOTICS M Compact induction motor 1000rpm, 22kW, 210Nm, 55A, 300V 1150rpm, 25kW, 208Nm, 55A, 343V 1350rpm, 28kW, 198Nm, 52A, 400 V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6157,"ST",1,"MC",196,1,"1PH81631AD100BA1"]
["1PH8163-1AF22-2BB1","SIMOTICS M Compact induction motor 1500rpm, 37kW, 236Nm, 84A, 328V 1750rpm, 43 kW, 235Nm, 84A, 380 V 2000rpm, 49kW, 234Nm, 84A, 430V water cooling Degree of protection IP65 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",8580,"ST",1,"MC",229,1,"1PH81631AF222BB1"]
["1PH8163-1DB03-1LB1","SIMOTICS M Compact induction motor 400rpm, 9.5kW 227Nm, 30 A, 260V 500rpm, 12kW 229Nm, 30 A, 325V 600rpm, 14.5kW 231Nm, 30 A, 370V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",9272,"ST",1,"MC",196,1,"1PH81631DB031LB1"]
["1PH8163-1DD03-2FA1","SIMOTICS M Compact induction motor 1000rpm, 22kW, 210Nm, 55A, 300V 1150rpm, 25kW, 208Nm, 55A, 343V 1350rpm, 28kW, 198Nm, 52A, 400 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: INCREASED RADIAL FORCES, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8759,"ST",1,"MC",196,1,"1PH81631DD032FA1"]
["1PH8163-1DF02-1GA1","SIMOTICS M Compact induction motor 1500rpm, 30 kW, 191Nm, 71A, 319V 1750rpm, 34kW, 186Nm, 70A, 366V 2000rpm, 37kW, 177Nm, 68A, 416V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8262,"ST",1,"MC",196,1,"1PH81631DF021GA1"]
["1PH8163-1DG00-0FA1","SIMOTICS M Compact induction motor 2000rpm, 36kW, 172Nm, 83A, 324V 2300rpm, 38 kW, 158Nm, 78A, 370V 2650rpm, 40kW, 144Nm, 76A, 390V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: INCREASED RADIAL FORCES, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7853,"ST",1,"MC",196,1,"1PH81631DG000FA1"]
["1PH8163-1DG12-0GA1","SIMOTICS M Compact induction motor 2000rpm, 36kW, 172Nm, 83A, 324V 2300rpm, 38 kW, 158Nm, 78A, 370V 2650rpm, 40kW, 144Nm, 76A, 390V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8053,"ST",1,"MC",196,1,"1PH81631DG120GA1"]
["1PH8163-1HB10-2CC1","SIMOTICS M Compact induction motor 400rpm, 9.5kW 227Nm, 30 A, 260V 500rpm, 12kW 229Nm, 30 A, 325V 600rpm, 14.5kW 231Nm, 30 A, 370V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",7000,"ST",1,"MC",196,1,"1PH81631HB102CC1"]
["1PH8163-1HD02-1BA2","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 22KW,210NM, 55A, 300V 1150RPM, 25KW,208NM, 55A, 343V 1350RPM, 28KW, 198NM, 52A, 400V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) TEMPERATURE SENSOR Pt1000 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7475,"ST",1,"MC",196,1,"1PH81631HD021BA2"]
["1PH8163-1HF10-1GB1","SIMOTICS M Compact induction motor 1500rpm, 30 kW, 191Nm, 71A, 319V 1750rpm, 34kW, 186Nm, 70A, 366V 2000rpm, 37kW, 177Nm, 68A, 416V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",6485,"ST",1,"MC",196,1,"1PH81631HF101GB1"]
["1PH8163-1HF22-2CC1","SIMOTICS M Compact induction motor 1500rpm, 37kW, 236Nm, 84A, 328V 1750rpm, 43 kW, 235Nm, 84A, 380 V 2000rpm, 49kW, 234Nm, 84A, 430V water cooling Degree of protection IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",9214,"ST",1,"MC",229,1,"1PH81631HF222CC1"]
["1PH8163-1JD13-0CA1","SIMOTICS M Compact induction motor 1000rpm, 22kW, 210Nm, 55A, 300V 1150rpm, 25kW, 208Nm, 55A, 343V 1350rpm, 28kW, 198Nm, 52A, 400 V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7937,"ST",1,"MC",196,1,"1PH81631JD130CA1"]
["1PH8163-1JF20-0BB1","SIMOTICS M Compact induction motor 1500rpm, 37kW, 236Nm, 84A, 328V 1750rpm, 43 kW, 235Nm, 84A, 380 V 2000rpm, 49kW, 234Nm, 84A, 430V water cooling Degree of protection IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",8549,"ST",1,"MC",229,1,"1PH81631JF200BB1"]
["1PH8163-1JF23-2CB1","SIMOTICS M Compact induction motor 1500rpm, 37kW, 236Nm, 84A, 328V 1750rpm, 43 kW, 235Nm, 84A, 380 V 2000rpm, 49kW, 234Nm, 84A, 430V water cooling Degree of protection IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",9664,"ST",1,"MC",229,1,"1PH81631JF232CB1"]
["1PH8163-1MF23-1LC1","SIMOTICS M Compact induction motor 1500rpm, 37kW, 236Nm, 84A, 328V 1750rpm, 43 kW, 235Nm, 84A, 380 V 2000rpm, 49kW, 234Nm, 84A, 430V water cooling Degree of protection IP65 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",10065,"ST",1,"MC",229,1,"1PH81631MF231LC1"]
["1PH8164-2DL23-2BC1","SIMOTICS M Compact synchronous motor 2500rpm, 88kW 335Nm, 165A, 355V 2800rpm, 93kW 315Nm, 156A, 395V 3000rpm, 96kW 305Nm, 150 A, 420V water cooling Degree of protection IP65 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",16437,"ST",1,"MC",224,1,"1PH81642DL232BC1"]
["1PH8165-1AF00-2QA1","SIMOTICS M Compact induction motor 1500rpm, 37kW, 236Nm, 78A, 350 V 1750rpm, 41kW, 224Nm, 76A, 400 V 2000rpm, 45kW, 215Nm, 75 A, 440 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: ADVANCED LIFETIME VIBRATION SEVERITY S/A SHAFT A. FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7521,"ST",1,"MC",230,1,"1PH81651AF002QA1"]
["1PH8165-1AF20-0BB1","SIMOTICS M Compact induction motor 1500rpm, 46 kW 293Nm, 104A, 330V 1750rpm, 53kW 289Nm, 104A, 374V 2000rpm, 60kW 287Nm, 103A, 426V water cooling Degree of protection IP65 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",9300,"ST",1,"MC",264,1,"1PH81651AF200BB1"]
["1PH8165-1DD00-0BB1","SIMOTICS M Compact induction motor 1000rpm, 28kW, 267Nm, 71A, 292V 1150rpm, 31kW, 257Nm, 69A, 333V 1350rpm, 34kW, 241Nm, 66A, 387V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",8253,"ST",1,"MC",230,1,"1PH81651DD000BB1"]
["1PH8165-1DD10-0CB1","SIMOTICS M Compact induction motor 1000rpm, 28kW, 267Nm, 71A, 292V 1150rpm, 31kW, 257Nm, 69A, 333V 1350rpm, 34kW, 241Nm, 66A, 387V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",8462,"ST",1,"MC",230,1,"1PH81651DD100CB1"]
["1PH8165-1DF02-1FC1","SIMOTICS M Compact induction motor 1500rpm, 37kW, 236Nm, 78A, 350 V 1750rpm, 41kW, 224Nm, 76A, 400 V 2000rpm, 45kW, 215Nm, 75 A, 440 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: INCREASED RADIAL FORCES, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",9351,"ST",1,"MC",230,1,"1PH81651DF021FC1"]
["1PH8165-1DF03-1DB1","SIMOTICS M Compact induction motor 1500rpm, 37kW, 236Nm, 78A, 350 V 1750rpm, 41kW, 224Nm, 76A, 400 V 2000rpm, 45kW, 215Nm, 75 A, 440 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE SR/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",9466,"ST",1,"MC",230,1,"1PH81651DF031DB1"]
["1PH8165-1DG00-1BC1","SIMOTICS M Compact induction motor 2000rpm, 41kW, 196Nm, 88A, 350 V 2300rpm, 44 kW, 183Nm, 85A, 394V 2650rpm, 50 kW, 180Nm, 85A, 440 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",8462,"ST",1,"MC",230,1,"1PH81651DG001BC1"]
["1PH8165-1DG10-2BB1","SIMOTICS M Compact induction motor 2000rpm, 41kW, 196Nm, 88A, 350 V 2300rpm, 44 kW, 183Nm, 85A, 394V 2650rpm, 50 kW, 180Nm, 85A, 440 V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",8462,"ST",1,"MC",230,1,"1PH81651DG102BB1"]
["1PH8165-1FF00-2CA1","SIMOTICS M Compact induction motor 1500rpm, 37kW, 236Nm, 78A, 350 V 1750rpm, 41kW, 224Nm, 76A, 400 V 2000rpm, 45kW, 215Nm, 75 A, 440 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9647,"ST",1,"MC",230,1,"1PH81651FF002CA1"]
["1PH8165-1HD00-1BA1","SIMOTICS M Compact induction motor 1000rpm, 28kW, 267Nm, 71A, 292V 1150rpm, 31kW, 257Nm, 69A, 333V 1350rpm, 34kW, 241Nm, 66A, 387V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7383,"ST",1,"MC",230,1,"1PH81651HD001BA1"]
["1PH8165-1HF12-0CA1","SIMOTICS M Compact induction motor 1500rpm, 37kW, 236Nm, 78A, 350 V 1750rpm, 41kW, 224Nm, 76A, 400 V 2000rpm, 45kW, 215Nm, 75 A, 440 V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8080,"ST",1,"MC",230,1,"1PH81651HF120CA1"]
["1PH8165-1HF20-0BA1","SIMOTICS M Compact induction motor 1500rpm, 46 kW 293Nm, 104A, 330V 1750rpm, 53kW 289Nm, 104A, 374V 2000rpm, 60kW 287Nm, 103A, 426V water cooling Degree of protection IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9725,"ST",1,"MC",264,1,"1PH81651HF200BA1"]
["1PH8165-1HG10-2BA1","SIMOTICS M Compact induction motor 2000rpm, 41kW, 196Nm, 88A, 350 V 2300rpm, 44 kW, 183Nm, 85A, 394V 2650rpm, 50 kW, 180Nm, 85A, 440 V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7383,"ST",1,"MC",230,1,"1PH81651HG102BA1"]
["1PH8165-1JF03-2BB1","SIMOTICS M Compact induction motor 1500rpm, 37kW, 236Nm, 78A, 350 V 1750rpm, 41kW, 224Nm, 76A, 400 V 2000rpm, 45kW, 215Nm, 75 A, 440 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",8529,"ST",1,"MC",230,1,"1PH81651JF032BB1"]
["1PH8165-1JF23-2BB1","SIMOTICS M Compact induction motor 1500rpm, 46 kW 293Nm, 104A, 330V 1750rpm, 53kW 289Nm, 104A, 374V 2000rpm, 60kW 287Nm, 103A, 426V water cooling Degree of protection IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",11081,"ST",1,"MC",264,1,"1PH81651JF232BB1"]
["1PH8165-1MF03-1LC1","SIMOTICS M Compact induction motor 1500rpm, 37kW, 236Nm, 78A, 350 V 1750rpm, 41kW, 224Nm, 76A, 400 V 2000rpm, 45kW, 215Nm, 75 A, 440 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",9140,"ST",1,"MC",230,1,"1PH81651MF031LC1"]
["1PH8165-1MF13-2CA1","SIMOTICS M Compact induction motor 1500rpm, 37kW, 236Nm, 78A, 350 V 1750rpm, 41kW, 224Nm, 76A, 400 V 2000rpm, 45kW, 215Nm, 75 A, 440 V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8644,"ST",1,"MC",230,1,"1PH81651MF132CA1"]
["1PH8165-2FF03-1CA1","SIMOTICS M Compact synchronous motor 1500rpm, 61kW 390Nm, 119A, 340V 1750rpm, 69kW 375Nm, 115A, 395V 2000rpm, 74kW 355Nm, 110 A, 445V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",18035,"ST",1,"MC",218,1,"1PH81652FF031CA1"]
["1PH8166-1AF20-2CC1","SIMOTICS M Compact induction motor 1500rpm, 52kW 331Nm, 116A, 332V 1750rpm, 61kW 333Nm, 116A, 381V 2000rpm, 68kW 325Nm, 116A, 426V water cooling Degree of protection IP65 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",10647,"ST",1,"MC",269,1,"1PH81661AF202CC1"]
["1PH8166-1FG23-2LC1","SIMOTICS M Compact induction motor 2000rpm, 64kW 306Nm, 125 A, 376V 2300rpm, 72kW 299Nm, 124A, 420V 2650rpm, 83kW 299Nm, 125 A, 460 V water cooling Degree of protection IP65 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",14320,"ST",1,"MC",269,1,"1PH81661FG232LC1"]
["1PH8166-1MF23-0BA1","SIMOTICS M Compact induction motor 1500rpm, 52kW 331Nm, 116A, 332V 1750rpm, 61kW 333Nm, 116A, 381V 2000rpm, 68kW 325Nm, 116A, 426V water cooling Degree of protection IP65 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",11706,"ST",1,"MC",269,1,"1PH81661MF230BA1"]
["1PH8184-1DB00-1CA1","SIMOTICS M Compact induction motor 400 rpm, 16.3kW 389Nm, 49A, 271V 500 rpm, 20.5kW 392Nm, 49A, 335V 600 rpm, 25kW 398Nm, 49A, 410V forced ventilation Direction of air flow DE-->NDE Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IMB6, IMB7, IMB8, IMV6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD VIBRATION SEVERITY GRADE S/A SHAFT A.FLANGE ACCURACY GR.R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",11352,"ST",1,"MC",350,1,"1PH81841DB001CA1"]
["1PH8184-1DL20-0BA1","SIMOTICS M Compact induction motor 2500rpm, 95kW 363Nm, 196A, 340V 2900rpm, 102kW 336Nm, 185A, 395V 3400rpm, 100 kW 281Nm, 158A, 460 V water cooling Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IMB6, IMB7, IMB8, IMV6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD VIBRATION SEVERITY GRADE R/A; SHAFT A.FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",14804,"ST",1,"MC",340,1,"1PH81841DL200BA1"]
["1PH8186-1DL03-1CA1","SIMOTICS M Compact induction motor 2500rpm, 106kW 405Nm, 230A, 335V 2900rpm, 101kW 333Nm, 198A, 385 V 3400RPM, 81kW 228Nm, 158A, 455V forced ventilation Direction of air flow DE-->NDE Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 WITH FLANGE A450 (IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD VIBRATION SEVERITY GRADE S/A SHAFT A.FLANGE ACCURACY GR.R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",16575,"ST",1,"MC",422,1,"1PH81861DL031CA1"]
["1PH8224-1DC00-0AC1","SIMOTICS M Compact induction motor 700 rpm, 55kW, 750Nm, 136A, 310V 800 rpm, 57kW, 681Nm, 126A, 350 V 1000 rpm, 71kW, 678Nm, 126A, 425V forced ventilation Direction of air flow DE-->NDE Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IMB6, IMB7, IMB8, IMV6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD VIBRATION SEVERITY GRADE A; SHAFT A.FLANGE ACCURACY GR.N TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION RIGHT",18062,"ST",1,"MC",610,1,"1PH82241DC000AC1"]
["1PH8224-1DF03-0CA1","SIMOTICS M Compact induction motor 1500rpm, 95kW, 605Nm, 200 A, 340V 1750rpm, 110 kW, 600Nm, 198A, 395V 2000rpm, 124kW, 592Nm, 196A, 460 V forced ventilation Direction of air flow DE-->NDE Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 WITH FLANGE A550 (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD VIBRATION SEVERITY GRADE S/A SHAFT A.FLANGE ACCURACY GR.R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",20404,"ST",1,"MC",610,1,"1PH82241DF030CA1"]
["1PH8228-1DD00-2FD1","SIMOTICS M Compact induction motor 1000rpm, 113kW 1079Nm, 235A, 340V 1150rpm, 129kW 1071Nm, 235A, 390V 1350rpm, 147kW 1040Nm, 225 A, 460 V forced ventilation Direction of air flow DE-->NDE Degree of protection IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IMB6, IMB7, IMB8, IMV6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: GREATER CANTILEVER FORCES; VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE D-END SIGNAL CONNECTION RIGHT",29259,"ST",1,"MC",870,1,"1PH82281DD002FD1"]
["6AU1810-1BA51-0XE0","SIMOTION ENGINEERING SYSTEM SCOUT AND SCOUT TIA V5.1 UPGRADE DVD INCL. STARTER, RUNTIME, TECHN., DOCUMENTATION, UTILITIES FOR FREE",659,"ST",1,"MC",0.01,1,"6AU18101BA510XE0"]
["6AU1810-1HA24-1XE0","SINAMICS ENGINEERING SYSTEM SINAMICS DCC V2.4 SP1 UPGRADE LICENSE DCC FOR SINAMICS OPTION TO STARTER V4.5 SP1 DELIVERY ON DATA CARRIER DVD INCL: FLOATING LICENSE",321,"ST",1,"MC",0.01,1,"6AU18101HA241XE0"]
["6FX2001-2CB50","INCREM. ENCODER 6FX2001-2CB50 WITH RS 422 (TTL), 1500 P/R, SYNCHRO-FLANGE SHAFT 6MM OPERATING VOLTAGE: 5 V UNIVERSAL CABLE OUTLET AXIAL / RADIAL CABLE 1M WITH CONNECTOR",388,"ST",1,"MC",0.495,1,"6FX20012CB50"]
["6FX2001-3CB00","INCREM. ENCODER 6FX2001-3CB00 WITH 1-V-SINUS 1000 P/R, SYNCHROFLANGE, 6 MM SHAFT, OPERATING VOLTAGE 5 V AXIAL/RADIAL UNIVERSAL CABLE OUTLET CABLE 1M WITH CONNECTOR",388,"ST",1,"MC",0.49,1,"6FX20013CB00"]
["6FX2001-5FD13-0AA1","Absolute encoder single-turn 6FX2001-5FD13 ST22 bit with DRIVE-CLiQ; Synchronous flange; Shaft 6 mm",1352,"ST",1,"MC",0.7,1,"6FX20015FD130AA1"]
["6FX2002-1DC00-1BB0","Signal cable pre-assembled type: 6FX2002-1DC00 (SINAMICS Drive CLiQ) Connector IP20/IP20, without 24 V Length (m)= 0 + 10 + 1 + 0",186,"ST",1,"MC",0.83,1,"6FX20021DC001BB0"]
["6FX2002-1DC20-1DA0","Signal cable pre-assembled type: 6FX2002-1DC20 (SINAMICS Drive CLiQ) Connector IP67/IP67, without 24 V Length (m)= 0 + 30 + 0 + 0",366,"ST",1,"MC",2,1,"6FX20021DC201DA0"]
["6FX3002-2CT20-1AF0","Signal cable pre-assembled 6FX3002-2CT20-1AF0 for incr. encoder in S-1FL6 LI 3x 2x 0.20+2x2X0.25 C MOTION-CONNECT 300 UL/CSA Dmax=7.5 mm Length (m)=5 m",125,"ST",1,"MC",0.39200000000000002,1,"6FX30022CT201AF0"]
["6FX3002-5CK32-1AD0","Power cable pre-assembled 4x2.5; FOR MOTOR S-1FL6 LI 200V SH50 WITH V90 FRAMESIZE D MOTION-CONNECT 300 NO UL FOR MOTOR-SIDE CONNECTOR DMAX=9.7mm LENGTH=3M With straight connector",126,"ST",1,"MC",0.67,1,"6FX30025CK321AD0"]
["6FX5002-2AH11-1EA0","Signal cable pre-assembled type: 6FX5002-2AH11 (basis 6FX5002-2AH00-....) with integrated temperature cores UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm Length (m)= 0 + 40 + 0 + 0",476,"ST",1,"MC",4.9400000000000004,1,"6FX50022AH111EA0"]
["6FX5002-2CA20-1CJ0","signal cable pre-assembled type: 6FX5002-2CA20 (incr. encoder in motor AH20) 3x 2x 0.14+4x 0.14+2x 0.5+4x 0.22C with M17 connector UL/CSA DESINA MOTION-CONNECT 500 Dmax=9.9 mm; Length (m)= 0 + 20 + 8 + 0",439,"ST",1,"MC",3.3610000000000002,1,"6FX50022CA201CJ0"]
["6FX5002-2CF02-1AA5","Signal cable pre-assembled (resolver in motor) 3x 2x 0.14+4x 0.14+2x0.5 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm Length (m)= TYPE: 6FX5002-2CF02 LENGTH (M) = 0 + 0 + 0 + 0,5",132,"ST",1,"MC",0.3,1,"6FX50022CF021AA5"]
["6FX5002-2CF02-1DA5","Signal cable pre-assembled (resolver in motor) 3x 2x 0.14+4x 0.14+2x0.5 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm Length (m)= TYPE: 6FX5002-2CF02 LENGTH (M) = 0 + 30 + 0 + 0,5",328,"ST",1,"MC",3.33,1,"6FX50022CF021DA5"]
["6FX5002-2CG00-1CF0","Signal cable pre-assembled (810D/611D to incremental encoder) 4x 2x 0.34+4x 0.5 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm TYPE: 6FX5002-2CG00 LENGTH (M) = 0 + 20 + 5 + 0",243,"ST",1,"MC",3.16,1,"6FX50022CG001CF0"]
["6FX5002-2DC00-1HF0","Signal cable pre-assembled type: 6FX5002-2DC00 (SINAMICS Drive CLiQ) connector IP20/IP20, with 24 V MOTION-CONNECT 500 Length (m)= 0 + 70 + 5 + 0",622,"ST",1,"MC",6.0970000000000004,1,"6FX50022DC001HF0"]
["6FX5002-2DC10-1CF0","Signal cable pre-assembled type: 6FX5002-2DC10 (SINAMICS Drive CLiQ) connector IP20/IP67, with 24 V MOTION-CONNECT 500 Length (m)= 0 + 20 + 5 + 0",288,"ST",1,"MC",2.0619999999999998,1,"6FX50022DC101CF0"]
["6FX5002-2DC10-1JG0","Signal cable pre-assembled type: 6FX5002-2DC10 (SINAMICS Drive CLiQ) connector IP20/IP67, with 24 V MOTION-CONNECT 500 Length (m)= 0 + 80 + 6 + 0",717,"ST",1,"MC",7.0030000000000001,1,"6FX50022DC101JG0"]
["6FX5002-2DC20-1AG0","Signal cable pre-assembled type: 6FX5002-2DC20 (SINAMICS Drive CLiQ) connector IP67/IP67, with 24 V MOTION-CONNECT 500 Length (m)= 0 + 0 + 6 + 0",171,"ST",1,"MC",0.53800000000000003,1,"6FX50022DC201AG0"]
["6FX5002-2DC44-1CA0","DRIVE-CLiQ extension type: 6FX5002-2DC44 for base 6FX5002-2DC40-.... with 24 V socket and connector M17 Speed-connect female/ male speed-connect-ready MOTION-CONNECT 500 UL/CSA, DESINA Dmax=7.1 mm Length (m)= 0 + 20 + 0 + 0",295,"ST",1,"MC",1.6120000000000001,1,"6FX50022DC441CA0"]
["6FX5002-2EN20-1BF0","Signal cable pre-assembled Absolute encoder EnDat in the motor, SPEED-CONNECT M17 3x 2x 0.14+4x 0.14+2x0.5+ 4x 0.22 C MOTION-CONNECT 500 trailable, UL/CSA, DESINA Dmax=9.8 mm TYPE: 6FX5002-2EN20 LENGTH (M) = 0 + 10 + 5 + 0",326,"ST",1,"MC",2.2170000000000001,1,"6FX50022EN201BF0"]
["6FX5002-5CA05-1AE0","power cable, pre-assembled, Extension 4x 1.5 C connector Sz. 1 (1FT/1FK to 611/810D/SIMOVERT) UL/CSA, DESINA MOTION-CONNECT 500 Dmax=11.5 mm TYPE: 6FX5002-5CA05 LENGTH (M) = 0 + 0 + 4 + 0",250,"ST",1,"MC",0.79300000000000004,1,"6FX50025CA051AE0"]
["6FX5002-5CF14-1BA0","Power cable pre-assembled type: 6FX5002-5CF14 4x 1.5 C, SPEED-CONNECT Sz. 1.5 for SINAMICS S120 Combi MOTION-CONNECT 500 UL/CSA, DESINA Dmax=8.4 mm Length (m)= 0 + 10 0 0",283,"ST",1,"MC",1.6,1,"6FX50025CF141BA0"]
["6FX5002-5CG10-1DJ0","Power cable pre-assembled 4x 1.5 C SPEED-CONNECT connector Sz. 1 (SINAMICS AC Drive) UL/CSA DESINA MOTION-CONNECT 500 Dmax=8.4 mm TYPE: 6FX5002-5CG10 LENGTH (M) = + 0 + 30 + 8 + 0",300,"ST",1,"MC",4.8369999999999997,1,"6FX50025CG101DJ0"]
["6FX5002-5CG12-1BC0","Power cable pre-assembled 4x 2.5 C SPEED-CONNECT connector Sz. 1 for SINAMICS Power Module MOTION-CONNECT 500 UL/CSA DESINA Dmax=10 mm TYPE: 6FX5002-5CG12 LENGTH (M) = 0 + 10 + 2 + 0",201,"ST",1,"MC",2.468,1,"6FX50025CG121BC0"]
["6FX5002-5CG62-1CA0","Power cable pre-assembled 4x 10 C Speed connect connector Sz. 1.5 (SINAMICS AC Drive) UL/CSA DESINA MOTION-CONNECT 500 Dmax=20.0 mm TYPE: 6FX5002-5CG62 LENGTH (M) = + 0 + 20 + 0 + 0",564,"ST",1,"MC",13.97,1,"6FX50025CG621CA0"]
["6FX5002-5CN01-1CA0","Power cable pre-assembled 4x 1.5 C SPEED-CONNECT connector Sz. 1 (SINAMICS Motor Module) UL/CSA DESINA MOTION-CONNECT 500 Dmax=11.5 mm TYPE: 6FX5002-5CN01 LENGTH (M) = + 0 + 20 + 0 + 0",357,"ST",1,"MC",2.7160000000000002,1,"6FX50025CN011CA0"]
["6FX5002-5CN26-1DA0","Power cable pre-assembled TYPE 6FX5002-5CN26 4X1,5C, SPEED-CONNECT SIZE 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX=8.4 MM LENGTH (M) = + 0 + 30 + 0 + 0",369,"ST",1,"MC",4.1210000000000004,1,"6FX50025CN261DA0"]
["6FX5002-5CN54-1BA0","Power cable pre-assembled 4x 6 C SPEED-CONNECT connector Sz. 1.5 Ring cable lug (SINAMICS Motor Module) UL/CSA DESINA MOTION-CONNECT 500 Dmax=15.6 mm TYPE: 6FX5002-5CN54 LENGTH (M) = + 0 + 10 + 0 + 0",334,"ST",1,"MC",4.0940000000000003,1,"6FX50025CN541BA0"]
["6FX5002-5CS01-1BJ0","Power cable pre-assembled type: 6FX5002-5CS01 (1FT/1FK/1PH for SINAMICS) 4x 1.5 C, Connector Sz. 1/1.5 mm2 UL/CSA DESINA MOTION-CONNECT 500 Dmax=8.4 mm, Length (m)= 0 + 10 + 8 + 0",347,"ST",1,"MC",2.4740000000000002,1,"6FX50025CS011BJ0"]
["6FX5002-5CS01-1GF0","Power cable pre-assembled type: 6FX5002-5CS01 (1FT/1FK/1PH for SINAMICS) 4x 1.5 C, Connector Sz. 1/1.5 mm2 UL/CSA DESINA MOTION-CONNECT 500 Dmax=8.4 mm, Length (m)= 0 + 60 + 5 + 0",582,"ST",1,"MC",8.1609999999999996,1,"6FX50025CS011GF0"]
["6FX5002-5CS21-1EA0","power cable pre-assembled type: 6FX5002-5CS21 (1FT/1FK for SINAMICS) 4x 1.5 C, Connector Sz. 1.5/1.5 mm2 UL/CSA, DESINA MOTION-CONNECT 500 Dmax=15.5 mm; Length (m)= 0 + 40 + 0 + 0",528,"ST",1,"MC",5.3280000000000003,1,"6FX50025CS211EA0"]
["6FX5002-5CS31-1BG0","power cable pre-assembled type: 6FX5002-5CS31 (1FT/1FK for SINAMICS) 4x 2.5 C, Connector Sz. 1.5/2.5 mm2 UL/CSA, DESINA MOTION-CONNECT 500 Dmax=12.9 mm; Length (m)= 0 + 10 + 6 + 0",436,"ST",1,"MC",3.8159999999999998,1,"6FX50025CS311BG0"]
["6FX5002-5CS42-1AE7","Power cable pre-assembled type: 6FX5002-5CS42 (1FT/1FK for SINAMICS) 4x 4 C, Motor side Exposed core ends/4 mm2 UL/CSA, DESINA MOTION-CONNECT 500 Dmax=14.1 mm; Length (m)= 0 + 0 + 4 + 0,7",248,"ST",1,"MC",1.462,1,"6FX50025CS421AE7"]
["6FX5002-5DA05-1AD5","power cable, pre-assembled, Extension 4x 1.5+(2x1.5) C, Connector Sz. 1 (1FT/1FK to 611/810D/SIMOVERT) UL/CSA, DESINA MOTION-CONNECT 500 Dmax=13.1 mm TYPE: 6FX5002-5DA05 LENGTH (M) = 0 + 0 + 3 + 0,5",274,"ST",1,"MC",1.02,1,"6FX50025DA051AD5"]
["6FX5002-5DA30-1BA0","power cable, pre-assembled type: 6FX5002-5DA30 4x 1.5+(2x1.5) C, Connector Sz. 0.5 (1FK7 AH20 to Power Modules and AC/AC drives) UL/CSA DESINA MOTION-CONNECT 500 Dmax=10.8 mm, Length (m)= 0 + 10 + 0 + 0",226,"ST",1,"MC",2.29,1,"6FX50025DA301BA0"]
["6FX5002-5DG12-1EA0","Power cable pre-assembled 4x 2.5+(2x1.5) C C SPEED-CONNECT Sz. 1 for SINAMICS Power Module MOTION-CONNECT 500 UL/CSA DESINA Dmax=12.4 mm TYPE: 6FX5002-5DG12 LENGTH (M) = 0 + 40 + 0 + 0",534,"ST",1,"MC",10.199999999999999,1,"6FX50025DG121EA0"]
["6FX5002-5DG31-1AD0","power cable pre-assembled type: 6FX5002-5DG31 4x 2.5+(2x1.5) C, Connector Sz. 1.5 (SINAMICS AC Drive) UL/CSA, DESINA MOTION-CONNECT 500 Dmax=12.4 mm 0 + 0 + 3 + 0",249,"ST",1,"MC",1.1379999999999999,1,"6FX50025DG311AD0"]
["6FX5002-5DN05-1CA0","power cable, pre-assembled, Extension 4x 1.5+(2x1.5) C SPEED-CONNECT connector Sz. 1 (SIMODRIVE) UL/CSA DESINA MOTION-CONNECT 500 Dmax=13.1 mm TYPE: 6FX5002-5DN05 LENGTH (M) = + 0 + 20 + 0 + 0",400,"ST",1,"MC",4.6500000000000004,1,"6FX50025DN051CA0"]
["6FX5002-5DN06-1DC0","Power cable pre-assembled TYPE 6FX5002-5DN06 4X1.5, (2X1.5)C C CONNECTOR SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX = 10.8 MM LENGTH (M) = + 0 + 30 + 2 + 0",418,"ST",1,"MC",6.931,1,"6FX50025DN061DC0"]
["6FX5002-5DN51-1BJ0","Power cable pre-assembled 4x 6+(2x1.5) C SPEED-CONNECT connector Sz. 1.5 (SINAMICS Motor Module) UL/CSA DESINA MOTION-CONNECT 500 Dmax=17.6 mm TYPE: 6FX5002-5DN51 LENGTH (M) = + 0 + 10 + 8 + 0",652,"ST",1,"MC",9.2379999999999995,1,"6FX50025DN511BJ0"]
["6FX5002-5DS01-1AF5","Power cable pre-assembled type: 6FX5002-5DS01 (1FT/1FK/1PH for SINAMICS) 4x 1.5+(2x1.5) C Connector Sz. 1/1.5 mm2 UL/CSA DESINA MOTION-CONNECT 500 Dmax=13.1 mm, Length (m)= 0 + 0 + 5 + 0,5",325,"ST",1,"MC",1.5189999999999999,1,"6FX50025DS011AF5"]
["6FX5002-5DS21-1CH0","Power cable pre-assembled type: 6FX5002-5DS21 (1FT/1FK/1PH for SINAMICS) 4x 1.5+(2x1.5) C Connector Sz. 1.5/1.5 mm2 UL/CSA DESINA MOTION-CONNECT 500 Dmax=13.1 mm, Length (m)= 0 + 20 + 7 + 0",567,"ST",1,"MC",6.4409999999999998,1,"6FX50025DS211CH0"]
["6FX5002-5DS41-1CA0","Power cable pre-assembled type: 6FX5002-5DS41 (1FT/1FK/1PH for SINAMICS) 4x 4+(2x1.5) C Connector Sz. 1.5/4 mm2 UL/CSA DESINA MOTION-CONNECT 500 Dmax=15.4 mm, Length (m)= 0 + 20 + 0 + 0",622,"ST",1,"MC",7.3840000000000003,1,"6FX50025DS411CA0"]
["6FX5002-8QN04-1BA0","Single cable prefabricated 4G0.38+2x0.38+4x0.2 C SPEED-CONNECT M12 connector Cores with end sleeve Data cable with IX connector UL/CSA DESINA MOTION-CONNECT 500 Dmax.=9.7 mm, length(m)= 0 + 10 + 0 + 0",286,"ST",1,"MC",1.46,1,"6FX50028QN041BA0"]
["6FX5008-1BB11-6AA0","Power cable sold by the meter type: 6FX5008-1BB11 4x 1.5 C UL/CSA, DESINA MOTION-CONNECT 500 Type of delivery: Disposable drum Dmax=8.4 mm, Length (m)=500",2976,"ST",1,"MC",90,1,"6FX50081BB116AA0"]
["6FX5008-1BB35-1AJ0","Power cable sold by the meter type: 6FX5008-1BB35 4x 35 C UL/CSA, DESINA MOTION-CONNECT 500 Type of delivery: up to 14 m ring from 15 m drum Dmax=31.5 mm, Length (m)= 0 +  0 + 8 + 0",491,"ST",1,"MC",14.961,1,"6FX50081BB351AJ0"]
["6FX5008-1BB41-1AG0","Power cable sold by the meter type: 6FX5008-1BB41 4x 6.0 C UL/CSA, DESINA MOTION-CONNECT 500 Type of delivery: to 69 m ring from 70 m drum Dmax=13.6 mm, Length (m)= 0 + 0 + 6 + 0",98.199999999999989,"ST",1,"MC",2.7610000000000001,1,"6FX50081BB411AG0"]
["6FX5008-1BB61-1FA0","Power cable sold by the meter type: 6FX5008-1BB61 4x 16 C UL/CSA, DESINA MOTION-CONNECT 500 Type of delivery: up to 29 m ring from 30 m drum Dmax=24.2 mm, Length (m)= 0 + 50 + 0 + 0",1488,"ST",1,"MC",55.000999999999998,1,"6FX50081BB611FA0"]
["6FX5012-2CF02-1AJ0","Signal cable pre-assembled (resolver in motor) 3x 2x 0.14+4x 0.14+2x0.5 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm Length (m)= TYPE: 6FX5012-2CF02 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = 0 + 0 + 8 + 0",177,"ST",1,"MC",1.0569999999999999,1,"6FX50122CF021AJ0"]
["6FX5012-5DN01-1DA0","Power cable pre-assembled 4x 1.5+(2x1.5) C SPEED-CONNECT connector Sz. 1 (SINAMICS Motor Module) UL/CSA DESINA MOTION-CONNECT 500 Dmax=10.8 mm TYPE: 6FX5012-5DN01 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = + 0 + 30 + 0 + 0",513,"ST",1,"MC",6.9089999999999998,1,"6FX50125DN011DA0"]
["6FX5012-5DS01-1DA0","Power cable pre-assembled type: 6FX5012-5DS01 (1FT/1FK/1PH for SINAMICS) 4x 1.5+(2x1.5) C Connector Sz. 1/1.5 mm2 UL/CSA DESINA MOTION-CONNECT 500 Module side: contacts crimped Connector housing enclosed; Dmax=13.1 mm, Length (m)= 0 + 30 + 0 + 0",521,"ST",1,"MC",6.9089999999999998,1,"6FX50125DS011DA0"]
["6FX7002-5EA41-1CG0","power cable, pre-assembled type: 6FX7002-5EA41 4x 4+(4x 0.5) C, Connector Sz. 1.5 (1FN to 611) trailable UL/CSA DESINA MOTION-CONNECT 700 Dmax=16.6 mm, Length (m)= 0 + 20 + 6 + 0",937,"ST",1,"MC",11.05,1,"6FX70025EA411CG0"]
["6FX7002-5YP22-1AA5","power cable, pre-assembled Extension type: 6FX7002-5YP22 (1FN3 motors) Cable lugs/Sz. 1.5 EX Cell O, MC 700 4x 6+(4x 0.5) C; Length (m)= 0 + 0 + 0 + 0,5",263,"ST",1,"MC",0.624,1,"6FX70025YP221AA5"]
["6FX8002-1AA01-1AF0","Signal cable pre-assembled for RS-232-C Interfaces 4x (2x0.18) C MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=6.7 mm Length (m)= TYPE: 6FX8002-1AA01 LENGTH (M) = + 0 + 0 + 5 + 0",181,"ST",1,"MC",0.33500000000000002,1,"6FX80021AA011AF0"]
["6FX8002-2BA00-1BF0","Signal cable pre-assembled SIMODRIVE 611 for modulating valve 4x (2x0.34)+4x 0.5 C MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.3 mm Length (m)= TYPE: 6FX8002-2BA00 LENGTH (M) = 0 + 10 + 5 + 0",244,"ST",1,"MC",1.867,1,"6FX80022BA001BF0"]
["6FX8002-2CA24-1BF0","Signal cable extension type: 6FX8002-2CA24 for base 6FX8002-2CA20-.... with connector full thread M17 (3x 2x 0.14) C+4x 0.14+2x 0.5+4x 0.22 C MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.8 mm Length (m)= 0 + 10 + 5 + 0",409,"ST",1,"MC",2.2749999999999999,1,"6FX80022CA241BF0"]
["6FX8002-2CA31-1CJ0","Signal cable pre-assembled for incr. encoder with C/D tracks integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2CA31 LENGTH (M) = + 0 + 20 + 8 + 0",453,"ST",1,"MC",2.6110000000000002,1,"6FX80022CA311CJ0"]
["6FX8002-2CA31-1GB1","Signal cable pre-assembled for incr. encoder with C/D tracks integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2CA31 LENGTH (M) = + 0 + 60 + 1 + 0,1",820,"ST",1,"MC",5.59,1,"6FX80022CA311GB1"]
["6FX8002-2CB54-1BB0","signal cable, pre-assembled Extension for incremental encoder TTL 5V, 6FX2001-2 4x (2x0.34)+4x 0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.3 mm Length (m)= TYPE: 6FX8002-2CB54 LENGTH (M) = 0 + 10 + 1 + 0",218,"ST",1,"MC",1.492,1,"6FX80022CB541BB0"]
["6FX8002-2CC80-1BF0","Signal cable pre-assembled Customer-specific Length (m)= TYPE: 6FX8002-2CC80 LENGTH (M) = 0 + 10 + 5 + 0",322,"ST",1,"MC",3.05,1,"6FX80022CC801BF0"]
["6FX8002-2CF02-1EA0","Signal cable pre-assembled For resolvers 3x (2x0.14) C+4x 0.14+2x0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.2 mm Length (m)= TYPE: 6FX8002-2CF02 LENGTH (M) = 0 + 40 + 0 + 0",579,"ST",1,"MC",4.1749999999999998,1,"6FX80022CF021EA0"]
["6FX8002-2CH00-1AF0","Signal cable pre-assembled for absolute encoder EnDat 6FX2001-5 3x (2x0.14) C+4x 0.14+2x0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.2 mm Length (m)= TYPE: 6FX8002-2CH00 LENGTH (M) = 0 + 0 + 5 + 0",203,"ST",1,"MC",0.64200000000000002,1,"6FX80022CH001AF0"]
["6FX8002-2DC00-1AB5","Signal cable pre-assembled type: 6FX8002-2DC00 DRIVE-CLiQ with 24 V Connector RJ45 IP20 on both sides MOTION-CONNECT 800PLUS released only up to 75 m length Dmax=7.1 mm Length (m)= 0 + 0 + 1 + 0,5",138,"ST",1,"MC",0.156,1,"6FX80022DC001AB5"]
["6FX8002-2DC00-1HA0","Signal cable pre-assembled type: 6FX8002-2DC00 DRIVE-CLiQ with 24 V Connector RJ45 IP20 on both sides MOTION-CONNECT 800PLUS released only up to 75 m length Dmax=7.1 mm Length (m)= 0 + 70 + 0 + 0",924,"ST",1,"MC",4.8140000000000001,1,"6FX80022DC001HA0"]
["6FX8002-2DC10-1AG8","signal cable, pre-assembled type: 6FX8002-2DC10 DRIVE-CLiQ with 24 V Connector RJ45 IP20 on module side and IP67 on motor side MOTION-CONNECT 800PLUS released only up to 75 m length Dmax=7.1 mm Length (m)= 0 + 0 + 6 + 0,8",188,"ST",1,"MC",0.49099999999999999,1,"6FX80022DC101AG8"]
["6FX8002-2DC10-1FB0","signal cable, pre-assembled type: 6FX8002-2DC10 DRIVE-CLiQ with 24 V Connector RJ45 IP20 on module side and IP67 on motor side MOTION-CONNECT 800PLUS released only up to 75 m length Dmax=7.1 mm Length (m)= 0 + 50 + 1 + 0",558,"ST",1,"MC",3.4969999999999999,1,"6FX80022DC101FB0"]
["6FX8002-2DC20-1CD0","Signal cable pre-assembled type: 6FX8002-2DC20 DRIVE-CLiQ with 24 V Connector RJ45 IP67 on both sides released only up to 75 m length Dmax=7.1 mm Length (m)= 0 + 20 + 3 + 0",342,"ST",1,"MC",1.6060000000000001,1,"6FX80022DC201CD0"]
["6FX8002-2DC36-1HA0","Signal cable pre-assembled Type: 6FX8002-2DC36 DRIVE-CLiQ with 24 V M12 female/ RJ45 IP67, MOTION-CONNECT 800PLUS UL/CSA, DESINA, Trailable Dmax=7.1 mm length (m)=70",796,"ST",1,"MC",4.45,1,"6FX80022DC361HA0"]
["6FX8002-2EQ10-1CK0","Signal cable pre-assembled for absolute encoder EnDat integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2EQ10 LENGTH (M) = 0 + 20 + 9 + 0",464,"ST",1,"MC",4.1609999999999996,1,"6FX80022EQ101CK0"]
["6FX8002-2EQ14-1AB8","Signal cable extension for base 6FX8002-2EQ10-.... 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2EQ14 LENGTH (M) = 0 + 0 + 1 + 0,8",195,"ST",1,"MC",0.43099999999999999,1,"6FX80022EQ141AB8"]
["6FX8002-2EQ14-1BH0","Signal cable extension for base 6FX8002-2EQ10-.... 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2EQ14 LENGTH (M) = 0 + 10 + 7 + 0",358,"ST",1,"MC",2.544,1,"6FX80022EQ141BH0"]
["6FX8002-4AA41-1AE0","Signal cable pre-assembled I/O devices for 840D and 8 2x (2x0.18) C MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=5.3 mm Length (m)= TYPE: 6FX8002-4AA41 LENGTH (M) = +0 +0 +4 +0",81.699999999999989,"ST",1,"MC",0.26,1,"6FX80024AA411AE0"]
["6FX8002-5CA05-1AD2","power cable extension 4x 1.5 C, connector Full-thread, size 1 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.5 mm, Length (m)= TYPE: 6FX8002-5CA05 LENGTH (M) = 0 + 0 + 3 + 0,2",296,"ST",1,"MC",0.72099999999999997,1,"6FX80025CA051AD2"]
["6FX8002-5CA58-1AF8","power cable extension 4x 6 C Connector full thread Sz. 1.5 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=14.9 mm Length (m)= TYPE: 6FX8002-5CA58 LENGTH (M) = 0 + 0 + 5 + 0,8",548,"ST",1,"MC",3.0350000000000001,1,"6FX80025CA581AF8"]
["6FX8002-5CF10-1AB0","Power cable pre-assembled type: 6FX8002-5CF10 4x 1.5 C, SPEED-CONNECT Sz. 1 for SINAMICS S120 Combi MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.5 mm, Length (m)= Dmax=9.5 mm, Length (m)= 0 + 0 + 1 + 0",138,"ST",1,"MC",0.32300000000000001,1,"6FX80025CF101AB0"]
["6FX8002-5CG22-1AJ0","Power cable pre-assembled 4x 1.5 C, SPEED-CONNECT Sz. 1.5 for SINAMICS S120 Power Module MOTION-CONNECT 800PLUS Trailable UL/CSA, DESINA Dmax=9.5 mm, Length (m)= TYPE: 6FX8002-5CG22 LENGTH (M) = + 0 + 0 + 8 + 0",314,"ST",1,"MC",1.615,1,"6FX80025CG221AJ0"]
["6FX8002-5CG61-1BA0","Power cable pre-assembled type: 6FX8002-5CG61 4x 10 C, Connector Sz. 1.5 (SINAMICS AC Drive) trailable UL/CSA DESINA MOTION-CONNECT 800 Dmax=19.4 mm Length (m)= + 0 + 10 + 0 + 0",577,"ST",1,"MC",6.6109999999999998,1,"6FX80025CG611BA0"]
["6FX8002-5CN06-1BF0","Power cable pre-assembled TYPE 6FX8002-5CN06 4X1,5 C, SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=9.5 MM LENGTH (M) = + 0 + 10 + 5 + 0",367,"ST",1,"MC",2.4500000000000002,1,"6FX80025CN061BF0"]
["6FX8002-5CN11-1BC5","Power cable pre-assembled 4x 2.5 C SPEED-CONNECT connector Sz. 1 for SINAMICS S120 Motor Module Booksize MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=11 mm Length (m)= TYPE: 6FX8002-5CN11 LENGTH (M) = 0 + 10 + 2 + 0,5",478,"ST",1,"MC",3.4350000000000001,1,"6FX80025CN111BC5"]
["6FX8002-5CN26-1BA5","Power cable pre-assembled TYPE 6FX8002-5CN26 4X1,5C, SPEED-CONNECT SIZE 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=9.5 MM LENGTH (M) = + 0 + 10 + 0 + 0.5",383,"ST",1,"MC",2.069,1,"6FX80025CN261BA5"]
["6FX8002-5CN51-1BA0","Power cable pre-assembled 4x 6 C SPEED-CONNECT connector Sz. 1.5 for SINAMICS S120 Motor Module MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=14.9 mm Length (m)= TYPE: 6FX8002-5CN51 LENGTH (M) = + 0 + 10 + 0 + 0",604,"ST",1,"MC",4.6139999999999999,1,"6FX80025CN511BA0"]
["6FX8002-5CN56-1BE0","Power cable pre-assembled TYPE 6FX8002-5CN56 4X6 C CONNECTOR SPEED-CONNECT S. 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=14.9 MM LENGTH (M) = + 0 + 10 + 4 + 0",545,"ST",1,"MC",6.0590000000000002,1,"6FX80025CN561BE0"]
["6FX8002-5CQ38-1BA5","power cable extension 4x 2.5 C SPEED-CONNECT connector Sz. 1.5 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=11 mm Length (m)= TYPE: 6FX8002-5CQ38 LENGTH (M) = 0 + 10 + 0 + 0,5",559,"ST",1,"MC",2.9889999999999999,1,"6FX80025CQ381BA5"]
["6FX8002-5CR10-1AF0","Power cable pre-assembled type: 6FX8002-5CR10 4x 2.5 C Screw connection M25/1PH808. for SINAMICS S120 Power Module and Motor Mod. Booksize Compact MOTION-CONNECT 800PLUS UL/CSA, DESINA Dmax=11 mm Length (m)= 0 + 0 + 5 + 0",262,"ST",1,"MC",1.647,1,"6FX80025CR101AF0"]
["6FX8002-5CS01-1BK0","Power cable pre-assembled type: 6FX8002-5CS01 4x 1.5 C, connector Full-thread, size 1 for SINAMICS S120 Motor Module MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.5 mm, Length (m)= 0 + 10 + 9 + 0",527,"ST",1,"MC",3.202,1,"6FX80025CS011BK0"]
["6FX8002-5CS01-1ED5","Power cable pre-assembled type: 6FX8002-5CS01 4x 1.5 C, connector Full-thread, size 1 for SINAMICS S120 Motor Module MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.5 mm, Length (m)= 0 + 40 + 3 + 0,5",860,"ST",1,"MC",7,1,"6FX80025CS011ED5"]
["6FX8002-5CS21-1AE0","Power cable pre-assembled type: 6FX8002-5CS21 4x 1.5 C, connector Full thread Sz. 1.5 for SINAMICS S120 Motor Module MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.5 mm, Length (m)= 0 + 0 + 4 + 0",403,"ST",1,"MC",1.069,1,"6FX80025CS211AE0"]
["6FX8002-5CS24-1AK0","Power cable pre-assembled type: 6FX8002-5CS24 4x 16 C Connector full thread Sz. 1.5 for SINAMICS S120 Motor Module Booksize MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=22.3 mm Length (m)= 0 + 0 + 9 + 0",546,"ST",1,"MC",8.83,1,"6FX80025CS241AK0"]
["6FX8002-5CS41-1AD8","Power cable pre-assembled type: 6FX8002-5CS41 4x 4 C Connector full thread Sz. 1.5 for SINAMICS S120 Motor Module Booksize MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=12.3 mm Length (m)= 0 + 0 + 3 + 0,8",433,"ST",1,"MC",1.64,1,"6FX80025CS411AD8"]
["6FX8002-5CS41-1HF0","Power cable pre-assembled type: 6FX8002-5CS41 4x 4 C Connector full thread Sz. 1.5 for SINAMICS S120 Motor Module Booksize MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=12.3 mm Length (m)= 0 + 70 + 5 + 0",1840,"ST",1,"MC",23.997,1,"6FX80025CS411HF0"]
["6FX8002-5CS64-1BG0","Power cable pre-assembled type: 6FX8002-5CS64 (1FT/1FK/1PH for SINAMICS) 4x 10 C, Connector Sz. 1.5/ Ring cable lug UL/CSA DESINA, Trailable MOTION-CONNECT 800 Dmax=18.4 mm, Length (m)= 0 + 10 + 6 + 0",797,"ST",1,"MC",10.321,1,"6FX80025CS641BG0"]
["6FX8002-5CX28-1AB0","power cable extension 4x 16 C Connector full thread Sz. 3 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=22.3 mm Length (m)= TYPE: 6FX8002-5CX28 LENGTH (M) = 0 + 0 + 1 + 0",1705,"ST",1,"MC",2.8559999999999999,1,"6FX80025CX281AB0"]
["6FX8002-5DA28-1AG0","power cable extension 4x 1.5+(2x1.5) C, connector Full thread Sz. 1.5 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=12 mm, LONGUEUR (m)= TYPE: 6FX8002-5DA28 LENGTH (M) = 0 + 0 + 6 + 0",505,"ST",1,"MC",1.996,1,"6FX80025DA281AG0"]
["6FX8002-5DA38-1BJ0","power cable extension 4x 2.5+(2x1.5) C C Connector full thread Sz. 1.5 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=13.8 mm Length (m)= TYPE: 6FX8002-5DA38 LENGTH (M) = 0 + 10 + 8 + 0",755,"ST",1,"MC",5.9809999999999999,1,"6FX80025DA381BJ0"]
["6FX8002-5DG01-1BE5","Power cable pre-assembled type: 6FX8002-5DG01 4x 1.5+(2x1.5) C C, connector Connector full thread Sz. 1 for SINAMICS Power Module MOTION-CONNECT 800PLUS Dmax=12 mm, Length (m)= + 0 + 10 + 4 + 0,5",404,"ST",1,"MC",3.633,1,"6FX80025DG011BE5"]
["6FX8002-5DG11-1CF0","Power cable pre-assembled type: 6FX8002-5DG11 4x 2.5+(2x1.5) C C Connector full thread Sz. 1 for SINAMICS S120 Power Module and Motor Mod. Booksize Compact MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=13.8 mm Length (m)= + 0 + 20 + 5 + 0",636,"ST",1,"MC",6.1180000000000003,1,"6FX80025DG111CF0"]
["6FX8002-5DG41-1CF0","Power cable pre-assembled type: 6FX8002-5DG41 4x 4+(2x1.5) C C Connector full thread Sz. 1.5 for SINAMICS S120 Power Module and Motor Mod. Booksize Compact MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=15.2 mm LΓ¤nge (m)= 0 + 20 + 5 + 0",971,"ST",1,"MC",10.395,1,"6FX80025DG411CF0"]
["6FX8002-5DG43-1EG0","Power cable pre-assembled type: 6FX8002-5DG43 (motors for Power Module and Motor Module) 4x 35+(2x1.5) C, Connector size 3 Core end cut off Length 300 mm UL/CSA DESINA MOTION-CONNECT 800 Dmax=32.0 mm Length (m)= Accessory kit: 4x cable lugs M8 1x cable lugs M6 1x spring-loaded terminal 0 + 40 + 6 + 0",6830,"ST",1,"MC",93.146000000000001,1,"6FX80025DG431EG0"]
["6FX8002-5DN01-1BD5","Power cable pre-assembled type: 6FX8002-5DN01 4x 1.5+(2x1.5) C C, connector SPEED-CONNECT Sz. 1 for SINAMICS S120 Motor Module MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=12 mm, Length (m)= 0 + 10 + 3 + 0,5",535,"ST",1,"MC",3.5249999999999999,1,"6FX80025DN011BD5"]
["6FX8002-5DN06-1BD5","Power cable pre-assembled TYPE 6FX8002-5DN06 4X1,5 , (2X1.5)C C CONNECTOR SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=12 MM LENGTH (M) = + 0 + 10 + 3 + 0.5",415,"ST",1,"MC",3.32,1,"6FX80025DN061BD5"]
["6FX8002-5DN21-1BD0","Power cable pre-assembled 4x 1.5+(2x1.5) C C, connector SPEED-CONNECT Sz. 1.5 for SINAMICS S120 Motor Module MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=12 mm, Length (m)= TYPE: 6FX8002-5DN21 LENGTH (M) = + 0 + 10 +  3 + 0",593,"ST",1,"MC",3.5960000000000001,1,"6FX80025DN211BD0"]
["6FX8002-5DN41-1FA0","Power cable pre-assembled 4x 4+(2x1.5) C C SPEED-CONNECT connector Sz. 1.5 for SINAMICS S120 Motor Module MOTION-CONNECT 800PLUS Trailable UL/CSA, DESINA Dmax=15.2 mm LΓ¤nge (m)= TYPE: 6FX8002-5DN41 LENGTH (M) = + 0 + 50 + 0 + 0",1586,"ST",1,"MC",20.302,1,"6FX80025DN411FA0"]
["6FX8002-5DN54-1AJ0","Power cable pre-assembled 4x 6+(2x1.5) C C SPEED-CONNECT connector Sz. 1.5 Ring cable lugs on module side for SINAMICS S120 Motor Module MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=17.3 mm LΓ¤nge (m)= TYPE: 6FX8002-5DN54 LENGTH (M) = + 0 + 0 + 8 + 0",484,"ST",1,"MC",4.5250000000000004,1,"6FX80025DN541AJ0"]
["6FX8002-5DS01-1BD3","Power cable pre-assembled type: 6FX8002-5DS01 4x 1.5+(2x1.5) C C, connector Full-thread, size 1 for SINAMICS S120 Motor Module MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=12 mm, Length (m)= 0 + 10 + 3 + 0,3",535,"ST",1,"MC",3.4769999999999999,1,"6FX80025DS011BD3"]
["6FX8002-5DS01-1DH0","Power cable pre-assembled type: 6FX8002-5DS01 4x 1.5+(2x1.5) C C, connector Full-thread, size 1 for SINAMICS S120 Motor Module MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=12 mm, Length (m)= 0 + 30 + 7 + 0",934,"ST",1,"MC",9.2119999999999997,1,"6FX80025DS011DH0"]
["6FX8002-5DS16-1BC0","Power cable pre-assembled TYPE 6FX8002-5DS16 4X2.5 , (2X1.5)C C CONNECTOR FULL THREAD SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=13.8 MM LENGTH (M) = + 0 + 10 + 2 + 0",416,"ST",1,"MC",3.589,1,"6FX80025DS161BC0"]
["6FX8002-5DS21-1BK5","Power cable pre-assembled type: 6FX8002-5DS21 4x 1.5+(2x1.5) C C, connector Full thread Sz. 1.5 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=12 mm, Length (m)= 0 + 10 + 9 + 0,5",715,"ST",1,"MC",5.1689999999999996,1,"6FX80025DS211BK5"]
["6FX8002-5DS36-1FA0","Power cable pre-assembled TYPE 6FX8002-5DS36 4X2.5 , (2X1.5)C C, CONNECTOR FULL THREAD SIZE 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=13.8 MM LENGTH (M) = + 0 + 50 + 0 + 0",1075,"ST",1,"MC",14.427,1,"6FX80025DS361FA0"]
["6FX8002-5DS41-1DA0","Power cable pre-assembled type: 6FX8002-5DS41 4x 4+(2x1.5) C C Connector full thread Sz. 1.5 for SINAMICS S120 Motor Module MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=15.2 mm LΓ¤nge (m)= 0 + 30 + 0 + 0",1103,"ST",1,"MC",12.362,1,"6FX80025DS411DA0"]
["6FX8002-5DS64-1CF0","Power cable pre-assembled type: 6FX8002-5DS64 4x 10+(2x1.5) C C Connector full thread Sz. 1.5 for SINAMICS S120 Motor Module Booksize Ring cable lug on module side MOTION-CONNECT 800PLUS trailable, UL/CSA DESINA Dmax=20.1 mm LΓ¤nge (m)= 0 + 20 + 5 + 0",1338,"ST",1,"MC",19.814,1,"6FX80025DS641CF0"]
["6FX8002-5DX38-1BC0","power cable extension 4x 25+(2x1.5) C C Connector full thread Sz. 3 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=27.6 mm Length (m)= TYPE: 6FX8002-5DX38 LENGTH (M) = 0 + 10 + 2 + 0",3305,"ST",1,"MC",20.094000000000001,1,"6FX80025DX381BC0"]
["6FX8002-7HY00-1BA0","Pre-assembled hybrid cable type: 6FX8002-7HY00 Power and DRIVE-CLiQ Outlet direction NDE/NDE for SINAMICS S120M MOTION-CONNECT 800PLUS Trailing type, UL/CSA DESINA Dmax=15 mm, Length (m)= 0 + 10 + 0 + 0",625,"ST",1,"MC",3.5609999999999999,1,"6FX80027HY001BA0"]
["6FX8002-7HY00-1FF5","Pre-assembled hybrid cable type: 6FX8002-7HY00 Power and DRIVE-CLiQ Outlet direction NDE/NDE for SINAMICS S120M MOTION-CONNECT 800PLUS Trailing type, UL/CSA DESINA Dmax=15 mm, Length (m)= 0 + 50 + 5 + 0,5",1726,"ST",1,"MC",19.486000000000001,1,"6FX80027HY001FF5"]
["6FX8002-7HY22-1CE2","Pre-assembled hybrid cable type: 6FX8002-7HY22 Power and DRIVE-CLiQ Outlet direction DE/DE for SINAMICS S120M MOTION-CONNECT 800PLUS Trailing type, UL/CSA DESINA Dmax=15 mm, Length (m)= 0 + 20 + 4 + 0,2",984,"ST",1,"MC",8.5280000000000005,1,"6FX80027HY221CE2"]
["6FX8008-1BA31-1BH0","Power cable sold by the meter type: 6FX8008-1BA31 4x 4+(2x1.5) C C MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=15.2 mm Type of delivery: up to 79 m ring from 80 drum Length (m)= 0 + 10 + 7 + 0",446,"ST",1,"MC",6.8010000000000002,1,"6FX80081BA311BH0"]
["6FX8008-1BA61-1BH0","Power cable sold by the meter type: 6FX8008-1BA61 4x 16+(2x1.5) C C MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=23.8 mm Type of delivery: up to 29 m ring from 30 m drum Length (m)= 0 + 10 + 7 + 0",1072,"ST",1,"MC",18.701000000000001,1,"6FX80081BA611BH0"]
["6FX8008-1BB41-1BE0","Power cable sold by the meter type: 6FX8008-1BB41 4x 6.0 C trailable UL/CSA DESINA MOTION-CONNECT 800PLUS Type of delivery: to 69 m ring from 70 m drum Dmax=14.9 mm, Length (m)= 0 + 10 + 4 + 0",372,"ST",1,"MC",6.0209999999999999,1,"6FX80081BB411BE0"]
["6FX8008-1BB51-1BE0","Power cable sold by the meter type: 6FX8008-1BB51 4x 10.0 C trailable UL/CSA DESINA MOTION-CONNECT 800PLUS Type of delivery: Disposable drum Dmax=18.2 mm, Length (m)= 0 + 10 + 4 + 0",524,"ST",1,"MC",8.8209999999999997,1,"6FX80081BB511BE0"]
["6FX8008-1BD41-6AA0","Signal cable sold by the meter type: 6FX8008-1BD41 3x (2x0.14) C+4x 0.14+2x0.5 C MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Type of delivery: Disposable drum Dmax=9.2 mm Length (m)=500",5997,"ST",1,"MC",61.5,1,"6FX80081BD416AA0"]
["6FX8012-2CF02-1BD0","Signal cable pre-assembled For resolvers 3x (2x0.14) C+4x 0.14+2x0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.2 mm Length (m)= TYPE: 6FX8012-2CF02 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = 0 + 10 + 3 + 0",286,"ST",1,"MC",1.448,1,"6FX80122CF021BD0"]
["6FX8012-5CN31-1BA0","Power cable pre-assembled 4x 2.5 C SPEED-CONNECT connector Sz. 1.5 for SINAMICS S120 Motor Module Booksize MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=11 mm Length (m)= TYPE: 6FX8012-5CN31 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = + 0 + 10 + 0 + 0",507,"ST",1,"MC",2.7519999999999998,1,"6FX80125CN311BA0"]
["6FX8012-5CS17-1AJ0","Power cable pre-assembled TYPE 6FX8012-5CS17 4X10 C CONNECTOR FULL THREAD SIZE 3 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES PREPARED CONDUCTORS, SINAMICS CONNECTOR INCLUDED MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=18.2 MM LENGTH (M) = + 0 + 0 + 8 + 0",918,"ST",1,"MC",6.4770000000000003,1,"6FX80125CS171AJ0"]
["6FX8012-5DN56-1CA0","Power cable pre-assembled TYPE 6FX8012-5DN56 4X6 , (2X1.5)C C CONNECTOR SPEED-CONNECT S 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES PREPARED CONDUCTORS, SINAMICS CONNECTOR INCLUDED MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=17.3 MM LENGTH (M) = + 0 + 20 + 0 + 0",771,"ST",1,"MC",10.56,1,"6FX80125DN561CA0"]
["6FX8042-2CA11-1AK0","Signal cable pre-assembled for incremental encoder sin/cos 1 Vpp 6FX2001-3 4x (2x0.34)+4x 0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.3 mm Length (m)= TYPE: 6FX8042-2CA11 MOTOR SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = + 0 + 0 + 9 + 0",187,"ST",1,"MC",1.2829999999999999,1,"6FX80422CA111AK0"]
["6SE7031-6EB87-2DA1","SINAMICS / SIMOVERT MASTERDRIVES BRAKING UNIT 510 -650 V DC, 100 KW PROTECTION IP20 DOCUMENTATION ON CD",3036,"ST",1,"MC",11.5,1,"6SE70316EB872DA1"]
["6SL3000-0DE25-5AA1","SINAMICS / SIMODRIVE HFD COMMUTATING REACTOR FOR 55KW ACTIVE LINE MODULE",3056,"ST",1,"MC",27,1,"6SL30000DE255AA1"]
["6SL3055-0AA00-3BA0","SINAMICS S120 TERMINAL MODULE CABINET TM54F WITHOUT DRIVE-CLIQ CABLE ADD ON BOARD FOR SINAMICS CONVERTORS WITH FAIL-SAFE IN- AND OUTPUTS",1197,"ST",1,"MC",0.66,1,"6SL30550AA003BA0"]
["6SL3130-6AE15-0AB1","SINAMICS S120 SMART LINE MODULE INPUT: 3AC 380-480V, 50/60HZ OUTPUT: 600VDC, 8.3A, 5KW FRAME SIZE: BOOKSIZE INTERNAL AIR COOLING INCL. CONTROL VOLTAGE ADAPTER MODULES PAINTED",1181,"ST",1,"MC",5.3,1,"6SL31306AE150AB1"]
["6SL3202-0AE21-8CA0","SINAMICS Output reactor FOR POWERMODULE FSB 3AC 380V-480V 18,5A",280,"ST",1,"MC",12.4,1,"6SL32020AE218CA0"]
["6SL3203-0BE22-0VA0","SINAMICS V EMC filter 200 V - 480 V  3-phase-AC, 50/6 for SINAMICS V70/V90 Size 60x260x130 (WxHxD)",261,"ST",1,"MC",2.8250000000000002,1,"6SL32030BE220VA0"]
["6SL3210-1PC22-8UL0","SINAMICS POWER MODULE PM240-2 WITHOUT FILTER WITH BUILT IN BRAKING CHOPPER 3AC200-240V +10/-10% 47-63HZ OUTPUT HIGH OVERLOAD: 5,5KW FOR 200% 3S,150% 57S,100% 240S AMBIENT TEMP -10 TO +50 DEG C OUTPUT LOW OVERLOAD: 7,5KW FOR 150% 3S,110% 57S,100% 240S AMBIENT TEMP -10 TO +40 DEG C 355 X 140 X 165 (HXWXD), FSC PROTECTION IP20 WITHOUT CONTROL UNIT AND PANEL APPROVED FOR CU FIRMWARE- VERSION V4.6",1169,"ST",1,"MC",4.8,1,"6SL32101PC228UL0"]
["6SL3210-1PE34-8AL0","SINAMICS G120/S120 POWER MODULE PM240-2 FSG C2 WITH BUILT IN BRAKING CHOPPER 3AC380-480V+10/-10% 47-63Hz OUTPUT HIGH OVERLOAD: 200kW FOR 200% 3S,150% 57S,100% 240S AMBIENT TEMP -20 bis +50 DEG C (HO) OUTPUT LOW OVERLOAD: 250kW FOR 150% 3S,110% 57S,100% 240S AMBIENT TEMP -20 bis +40 DEG C (LO) 1000x305x357 (HXWXD), FSG PROTECTION IP20 WITHOUT CONTROL UNIT AND PANEL APPROVED FOR CU FIRMWARE- Version V4.7 SP9 AND V5.1",22478,"ST",1,"MC",138,1,"6SL32101PE348AL0"]
["6SL3210-1RE28-8UL0","SINAMICS G120 POWER MODULE PM240P-2 UNFILTERED 3AC380-480V +10/-20% 47-63HZ OUTPUT HIGH OVERLOAD: 37KW FOR 150% 60S, 100% 240S; AMBIENT TEMP -20 TO +50 DEG C (HO) OUTPUT LOW OVERLOAD: 45kW FOR 135% 3S,110% 57S,100% 240S AMBIENT TEMP -20 TO +40 DEG C (LO) 551x 275x 237 (HXWXD), FSE PROTECTION IP20 WITHOUT CONTROL UNIT AND PANEL APPROVED FOR CU FIRMWARE- VERSION V4.7 SP6 HF1",5216,"ST",1,"MC",30.9,1,"6SL32101RE288UL0"]
["6SL3211-0AB15-5UA1","SINAMICS G110-CPM110 AC Drive, unfiltered 200-240V1AC+10/-10% 47-63Hz Analog input CT: 0.55kW; VT: 0.55kW CT overload: 150% 60s 150x 90x 131 (HxWxD) Degree of protection IP20 Ambient temperature -10+50 Β°C without BOP without RS485 interface",283,"ST",1,"MC",0.8,1,"6SL32110AB155UA1"]
["6SL3216-5BE17-5CV0","SINAMICS V20 380-480 V 3AC -15%/+10%  47-6 Rated power 0.75 kW with 150% overload for 60 sec. Integrated filter C3 I/O interface: 4 DI, 2 DQ, 2 AI, 1 AO Fieldbus: USS/Modbus RTU with built-in BOP Degree of protection IP20/UL open Size: Size A 90x150x115 (WxHxD) flat heat sink",413,"ST",1,"MC",1.2,1,"6SL32165BE175CV0"]
["6SL3220-2YE46-0AF0","SINAMICS G120X Rated power: 110 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C2 With Basic Operator Panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",9935,"ST",1,"MC",84,1,"6SL32202YE460AF0"]
["6SL3220-3YE26-0UF0","SINAMICS G120X Rated power: 11 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSC Degree of protection IP20 / UL open type Paint finish 3C2 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",1711,"ST",1,"MC",8.3000000000000007,1,"6SL32203YE260UF0"]
["6SL3260-4NA00-1VA5","SINAMICS V90 50-point setpoint signal cable Cable length: 0.5 m with connecting terminal",129,"ST",1,"MC",0.5,1,"6SL32604NA001VA5"]
["6SL3266-1EC00-0KA0","SINAMICS G120C SCREENING PLATE FOR FSC INCLUDES SCREENING PLATE AND MOUNTING ACCESSORIES",106,"ST",1,"MC",0.215,1,"6SL32661EC000KA0"]
["6SL3544-0NB02-1FA0","SINAMICS G110M Control Unit CU240M PN G PROFINET with M screw connection 4 DI, 2 DO, 2 AI, 1 F-DI PTC/KTY connection EM brake control Degree of protection IP66 Ambient temperature -10 to +55 Β°C 105x 171x 205 (HxWxD) without Power Module",799,"ST",1,"MC",1.75,1,"6SL35440NB021FA0"]
["6SL3562-6DF71-0RG1","DISTRIBUTED SERVO-DRIVE SINAMICS S120M AH63, M(0)=5Nm, N(N)=3000 RPM, INPUT: DC 600V ABSOLUTE ENCODER 20 BIT NATURAL AIR COOLING, IM B5, IM V1, IM V3 DEGREE OF PROTECTION: IP65 PLAIN SHAFT W/O HOLDING BRAKE",4532,"ST",1,"MC",12.2,1,"6SL35626DF710RG1"]
["1LE1001-0BA32-2JB4","SIMOTICS GP Motor type: 1AV2063A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 63M * 0.25 kW (50 Hz) 0.29kW(60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF115 (A140) 1 PTC thermistor for disconnection (2 terminals) Terminal box at top",219,"ST",1,"LVM",5,1,"1LE10010BA322JB4"]
["1LE1001-0CA32-1FA4","SIMOTICS GP Motor type: 1AV2073A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 71M * 0.55 kW (50 Hz) 0.63kW(60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF130 (A160) without motor protection Terminal box at top",243,"ST",1,"LVM",7,1,"1LE10010CA321FA4"]
["1LE1001-0DA23-3AB6","SIMOTICS GP Motor type: 1AV2082A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 80M * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 3, 1 PTC thermistor for disconnection (2 terminals) Terminal box lateral left",263,"ST",1,"LVM",9,1,"1LE10010DA233AB6"]
["1LE1001-0DA23-4GA6","SIMOTICS GP Motor type: 1AV2082A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 80M * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF165 (A200) without motor protection Terminal box lateral left",255,"ST",1,"LVM",9,1,"1LE10010DA234GA6"]
["1LE1001-0DA30-4FB5","SIMOTICS GP Motor type: 1AV2083A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 80M * 1.1kW (50 Hz) 1.27kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF165 (A200) 1 PTC thermistor for disconnection (2 terminals) Terminal box lateral right",302,"ST",1,"LVM",11,1,"1LE10010DA304FB5"]
["1LE1001-0DA33-3GA4","SIMOTICS GP Motor type: 1AV2083A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 80M * 1.1kW (50 Hz) 1.27kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF165 (A200) without motor protection Terminal box at top",286,"ST",1,"LVM",11,1,"1LE10010DA333GA4"]
["1LE1001-0DB22-1JA5","SIMOTICS GP Motor type: 1AV2082B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency 4-pole * Size 80M * 0.55kW (50 Hz) 60Hz: IEC 60034-30 0.63kW 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF165 (A200) without motor protection Terminal box lateral right",270,"ST",1,"LVM",10,1,"1LE10010DB221JA5"]
["1LE1001-0DB29-0FB4","SIMOTICS GP Motor type: 1AV2082B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency 4-pole * Size 80M * 0.55kW (50 Hz) 60Hz: IEC 60034-30 0.63kW 3 AC 60 Hz 220 VD/380 VY * 50 Hz power IM B 5, flange: FF165 (A200) 1 PTC thermistor for disconnection (2 terminals) Terminal box at top",270,"ST",1,"LVM",10,1,"1LE10010DB290FB4"]
["1LE1001-0DB32-2AC6","SIMOTICS GP Motor type: 1AV2083B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 80M * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 2 PTC thermistors for warning and shutdown (4 terminals) Terminal box lateral left",323,"ST",1,"LVM",11,1,"1LE10010DB322AC6"]
["1LE1001-0EA02-2AA5","SIMOTICS GP Motor type: 1AV2090A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 90S * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, without motor protection Terminal box lateral right",303,"ST",1,"LVM",13,1,"1LE10010EA022AA5"]
["1LE1001-0EA02-2AB6","SIMOTICS GP Motor type: 1AV2090A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 90S * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 1 PTC thermistor for disconnection (2 terminals) Terminal box lateral left",321,"ST",1,"LVM",13.000999999999999,1,"1LE10010EA022AB6"]
["1LE1001-0EA42-1FB6","SIMOTICS GP Motor type: 1AV2094A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 90L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF165 (A200) 1 PTC thermistor for disconnection (2 terminals) Terminal box lateral left",450,"ST",1,"LVM",15.000999999999999,1,"1LE10010EA421FB6"]
["1LE1001-0EA43-3AB5","SIMOTICS GP Motor type: 1AV2094A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 90L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 3, 1 PTC thermistor for disconnection (2 terminals) Terminal box lateral right",422,"ST",1,"LVM",15.000999999999999,1,"1LE10010EA433AB5"]
["1LE1001-0EB02-2AA6","SIMOTICS GP Motor type: 1AV2090B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 90S * 1.1kW (50 Hz) 1.27kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, without motor protection Terminal box lateral left",294,"ST",1,"LVM",13,1,"1LE10010EB022AA6"]
["1LE1001-0EB03-4AB6","SIMOTICS GP Motor type: 1AV2090B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 90S * 1.1kW (50 Hz) 1.27kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 1 PTC thermistor for disconnection (2 terminals) Terminal box lateral left",313,"ST",1,"LVM",13.000999999999999,1,"1LE10010EB034AB6"]
["1LE1001-0EB42-2JA4","SIMOTICS GP Motor type: 1AV2094B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 90L * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF165 (A200) without motor protection Terminal box at top",358,"ST",1,"LVM",16,1,"1LE10010EB422JA4"]
["1LE1001-0EB43-4FC5","SIMOTICS GP Motor type: 1AV2094B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 90L * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF165 (A200) 2 PTC thermistors for warning and shutdown (4 terminals) Terminal box lateral right",447,"ST",1,"LVM",16,1,"1LE10010EB434FC5"]
["1LE1001-0EC03-3GA4","SIMOTICS GP Motor type: 1AV2090C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 90S * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF165 (A200) without motor protection Terminal box at top",318,"ST",1,"LVM",13,1,"1LE10010EC033GA4"]
["1LE1001-0EC03-4GB6","SIMOTICS GP Motor type: 1AV2090C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 90S * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF165 (A200) 1 PTC thermistor for disconnection (2 terminals) Terminal box lateral left",335,"ST",1,"LVM",13.000999999999999,1,"1LE10010EC034GB6"]
["1LE1001-0EC43-4AB4","SIMOTICS GP Motor type: 1AV2094C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 60 Hz, P60: IE1 6-pole * Size 90L * 1.10kW (50 Hz) 1.27kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 1 PTC thermistor for disconnection (2 terminals) Terminal box at top",356,"ST",1,"LVM",16.001000000000001,1,"1LE10010EC434AB4"]
["1LE1001-1AA40-4FA5","SIMOTICS GP Motor type: 1AV2104A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 kW (60Hz), 50 Hz power 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF215 (A250) without motor protection Terminal box on RHS",519,"ST",1,"LVM",21,1,"1LE10011AA404FA5"]
["1LE1001-1AA43-3FB7","SIMOTICS GP Motor type: 1AV2104A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 kW (60Hz), 50 Hz power 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 5, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",592,"ST",1,"LVM",21,1,"1LE10011AA433FB7"]
["1LE1001-1AA43-4JB7","SIMOTICS GP Motor type: 1AV2104A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 kW (60Hz), 50 Hz power 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",573,"ST",1,"LVM",21,1,"1LE10011AA434JB7"]
["1LE1001-1AB40-4JA6","SIMOTICS GP Motor type: 1AV2104B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 100L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF215 (A250) without motor protection Terminal box on left-hand side",485,"ST",1,"LVM",21,1,"1LE10011AB404JA6"]
["1LE1001-1AB42-2GA7","SIMOTICS GP Motor type: 1AV2104B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 100L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF215 (A250) without motor protection Terminal box below",481,"ST",1,"LVM",21,1,"1LE10011AB422GA7"]
["1LE1001-1AB43-4GB7","SIMOTICS GP Motor type: 1AV2104B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 100L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",531,"ST",1,"LVM",21,1,"1LE10011AB434GB7"]
["1LE1001-1AB52-2JA7","SIMOTICS GP Motor type: 1AV2105B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF215 (A250) without motor protection Terminal box below",544,"ST",1,"LVM",25,1,"1LE10011AB522JA7"]
["1LE1001-1AB53-4JA5","SIMOTICS GP Motor type: 1AV2105B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF215 (A250) without motor protection Terminal box on RHS",544,"ST",1,"LVM",25,1,"1LE10011AB534JA5"]
["1LE1001-1AC42-2AB4","SIMOTICS GP Motor type: 1AV2104C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 100L * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",449,"ST",1,"LVM",25,1,"1LE10011AC422AB4"]
["1LE1001-1AC42-2GA4","SIMOTICS GP Motor type: 1AV2104C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 100L * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF215 (A250) without motor protection Terminal box at top",433,"ST",1,"LVM",25,1,"1LE10011AC422GA4"]
["1LE1001-1BA22-1FB7","SIMOTICS GP Motor type: 1AV2112A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",693,"ST",1,"LVM",27,1,"1LE10011BA221FB7"]
["1LE1001-1BA22-2GC5","SIMOTICS GP Motor type: 1AV2112A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF215 (A250) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",701,"ST",1,"LVM",27,1,"1LE10011BA222GC5"]
["1LE1001-1BB22-1AA4","SIMOTICS GP Motor type: 1AV2112B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, without motor protection Terminal box at top",599,"ST",1,"LVM",29,1,"1LE10011BB221AA4"]
["1LE1001-1BB22-1FA7","SIMOTICS GP Motor type: 1AV2112B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF215 (A250) without motor protection Terminal box below",689,"ST",1,"LVM",29,1,"1LE10011BB221FA7"]
["1LE1001-1BB23-4GB4","SIMOTICS GP Motor type: 1AV2112B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",664,"ST",1,"LVM",29,1,"1LE10011BB234GB4"]
["1LE1001-1BB23-3FB5","SIMOTICS GP Motor type: 1AV2112B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 5, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",739,"ST",1,"LVM",29,1,"1LE10011BB233FB5"]
["1LE1001-1BC22-1JB5","SIMOTICS GP Motor type: 1AV2112C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 112M, * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",671,"ST",1,"LVM",29,1,"1LE10011BC221JB5"]
["1LE1001-1BC23-4AC4","SIMOTICS GP Motor type: 1AV2112C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 112M, * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",586,"ST",1,"LVM",29,1,"1LE10011BC234AC4"]
["1LE1001-1CA00-4WB4","SIMOTICS GP Motor type: 1AV2130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF265 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",801,"ST",1,"LVM",39,1,"1LE10011CA004WB4"]
["1LE1001-1CA03-3AA4","SIMOTICS GP Motor type: 1AV2130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 3, without motor protection Terminal box at top",691,"ST",1,"LVM",39,1,"1LE10011CA033AA4"]
["1LE1001-1CA03-4AA6","SIMOTICS GP Motor type: 1AV2130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box on left-hand side",707,"ST",1,"LVM",39,1,"1LE10011CA034AA6"]
["1LE1001-1CA12-1JB6","SIMOTICS GP Motor type: 1AV2131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1052,"ST",1,"LVM",43,1,"1LE10011CA121JB6"]
["1LE1001-1CA12-2GC7","SIMOTICS GP Motor type: 1AV2131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",1054,"ST",1,"LVM",43,1,"1LE10011CA122GC7"]
["1LE1001-1CB02-1FA4","SIMOTICS GP Motor type: 1AV2130B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF265 (A300) without motor protection Terminal box at top",797,"ST",1,"LVM",42,1,"1LE10011CB021FA4"]
["1LE1001-1CB00-4GB4","SIMOTICS GP Motor type: 1AV2130B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",837,"ST",1,"LVM",42,1,"1LE10011CB004GB4"]
["1LE1001-1CB03-4GA5","SIMOTICS GP Motor type: 1AV2130B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF265 (A300) without motor protection Terminal box on RHS",813,"ST",1,"LVM",42,1,"1LE10011CB034GA5"]
["1LE1001-1CB09-0JA4","SIMOTICS GP Motor type: 1AV2130B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 60 Hz 440 VD * 60 Hz power IM B 35 * Flange: FF265 (A300) without motor protection Terminal box at top",799,"ST",1,"LVM",42,1,"1LE10011CB090JA4"]
["1LE1001-1CB22-2JB6","SIMOTICS GP Motor type: 1AV2132B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations to be considered! 4-pole * Size 132M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1084,"ST",1,"LVM",49,1,"1LE10011CB222JB6"]
["1LE1001-1CB23-4FB6","SIMOTICS GP Motor type: 1AV2132B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations to be considered! 4-pole * Size 132M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1082,"ST",1,"LVM",49,1,"1LE10011CB234FB6"]
["1LE1001-1CC02-2FA5","SIMOTICS GP Motor type: 1AV2130C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 132S, * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF265 (A300) without motor protection Terminal box on RHS",742,"ST",1,"LVM",38,1,"1LE10011CC022FA5"]
["1LE1001-1CB23-4FB7","SIMOTICS GP Motor type: 1AV2132B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations to be considered! 4-pole * Size 132M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1082,"ST",1,"LVM",49,1,"1LE10011CB234FB7"]
["1LE1001-1CC03-3FB6","SIMOTICS GP Motor type: 1AV2130C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 132S, * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 5, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",853,"ST",1,"LVM",38,1,"1LE10011CC033FB6"]
["1LE1001-1CC03-4JB6","SIMOTICS GP Motor type: 1AV2130C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 132S, * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",819,"ST",1,"LVM",38,1,"1LE10011CC034JB6"]
["1LE1001-1CC22-1WB5","SIMOTICS GP Motor type: 1AV2132C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 132M, * 4kW (50 Hz) 4.6 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 15 * Flange: FF265 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",1014,"ST",1,"LVM",43,1,"1LE10011CC221WB5"]
["1LE1001-1CC23-3GA7","SIMOTICS GP Motor type: 1AV2132C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 132M, * 4kW (50 Hz) 4.6 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF265 (A300) without motor protection Terminal box below",924,"ST",1,"LVM",43,1,"1LE10011CC233GA7"]
["1LE1001-1CC32-1FA6","SIMOTICS GP Motor type: 1AV2133C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 132M, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF265 (A300) without motor protection Terminal box on left-hand side",1130,"ST",1,"LVM",52,1,"1LE10011CC321FA6"]
["1LE1001-1CC32-1GB6","SIMOTICS GP Motor type: 1AV2133C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 132M, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1205,"ST",1,"LVM",52,1,"1LE10011CC321GB6"]
["1LE1001-1CC33-3FA6","SIMOTICS GP Motor type: 1AV2133C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 132M, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 5, flange: FF265 (A300) without motor protection Terminal box on left-hand side",1130,"ST",1,"LVM",52,1,"1LE10011CC333FA6"]
["1LE1001-1DA22-1GA5","SIMOTICS GP Motor type: 1AV2162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF300 (A350) without motor protection Terminal box on RHS",1326,"ST",1,"LVM",67,1,"1LE10011DA221GA5"]
["1LE1001-1DA22-2GB7","SIMOTICS GP Motor type: 1AV2162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1358,"ST",1,"LVM",67,1,"1LE10011DA222GB7"]
["1LE1001-1DA23-4GC4","SIMOTICS GP Motor type: 1AV2162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",1342,"ST",1,"LVM",67,1,"1LE10011DA234GC4"]
["1LE1001-1DA32-1AB5","SIMOTICS GP Motor type: 1AV2163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",1683,"ST",1,"LVM",75,1,"1LE10011DA321AB5"]
["1LE1001-1DA33-3AB7","SIMOTICS GP Motor type: 1AV2163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1683,"ST",1,"LVM",75,1,"1LE10011DA333AB7"]
["1LE1001-1DA33-4AC6","SIMOTICS GP Motor type: 1AV2163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",1679,"ST",1,"LVM",75,1,"1LE10011DA334AC6"]
["1LE1001-1DA42-2FA4","SIMOTICS GP Motor type: 1AV2164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations to be considered! 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",1869,"ST",1,"LVM",84,1,"1LE10011DA422FA4"]
["1LE1001-1DA42-2JC5","SIMOTICS GP Motor type: 1AV2164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations to be considered! 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",2048,"ST",1,"LVM",84,1,"1LE10011DA422JC5"]
["1LE1001-1DA43-4AC7","SIMOTICS GP Motor type: 1AV2164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations to be considered! 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",1969,"ST",1,"LVM",84,1,"1LE10011DA434AC7"]
["1LE1001-1DB22-1JB4","SIMOTICS GP Motor type: 1AV2162B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1383,"ST",1,"LVM",71,1,"1LE10011DB221JB4"]
["1LE1001-1DB23-4FC4","SIMOTICS GP Motor type: 1AV2162B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",1371,"ST",1,"LVM",71,1,"1LE10011DB234FC4"]
["1LE1001-1DB42-1AB7","SIMOTICS GP Motor type: 1AV2164B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 160L, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1699,"ST",1,"LVM",83,1,"1LE10011DB421AB7"]
["1LE1001-1DB42-2JC5","SIMOTICS GP Motor type: 1AV2164B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 160L, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",1775,"ST",1,"LVM",83,1,"1LE10011DB422JC5"]
["1LE1001-1DB43-3GB7","SIMOTICS GP Motor type: 1AV2164B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 160L, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1771,"ST",1,"LVM",83,1,"1LE10011DB433GB7"]
["1LE1001-1DC22-1FB4","SIMOTICS GP Motor type: 1AV2162C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 6-pole * Size 160M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1434,"ST",1,"LVM",77,1,"1LE10011DC221FB4"]
["1LE1001-1DC20-4FB7","SIMOTICS GP Motor type: 1AV2162C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 6-pole * Size 160M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1446,"ST",1,"LVM",77,1,"1LE10011DC204FB7"]
["1LE1001-1DC23-3GB4","SIMOTICS GP Motor type: 1AV2162C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 6-pole * Size 160M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1434,"ST",1,"LVM",77,1,"1LE10011DC233GB4"]
["1LE1001-1DC42-1FB6","SIMOTICS GP Motor type: 1AV2164C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 6-pole * Size 160L, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1964,"ST",1,"LVM",93,1,"1LE10011DC421FB6"]
["1LE1001-1DC42-2AA5","SIMOTICS GP Motor type: 1AV2164C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 6-pole * Size 160L, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, without motor protection Terminal box on RHS",1774,"ST",1,"LVM",93,1,"1LE10011DC422AA5"]
["1LE1002-0BA22-1AB4","SIMOTICS GP Motor type: 1AV1062A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) aluminum housing Standard efficiency IE1, 2-pole * Size 63M * 0.18kW (50 Hz) 0.21kW(60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B3 1 PTC thermistor for disconnection (2 terminals) Terminal box at top",156,"ST",1,"LVM",4,1,"1LE10020BA221AB4"]
["1LE1002-0BA23-4FA4","SIMOTICS GP Motor type: 1AV1062A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) aluminum housing Standard efficiency IE1, 2-pole * Size 63M * 0.18kW (50 Hz) 0.21kW(60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF115 (A140) Without motor protection Terminal box at top",146,"ST",1,"LVM",4,1,"1LE10020BA234FA4"]
["1LE1002-0CA33-4JC4","SIMOTICS GP Motor type: 1AV1073A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) aluminum housing Standard efficiency IE1, 2-pole * Size 71M * 0.55 kW (50 Hz) 0.63kW(60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF130 (A160) 2 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",250,"ST",1,"LVM",6,1,"1LE10020CA334JC4"]
["1LE1002-1CA03-4GA4","SIMOTICS GP Motor type: 1AV1130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing Standard efficiency IE1, 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF265 (A300) without motor protection Terminal box at top",602,"ST",1,"LVM",35,1,"1LE10021CA034GA4"]
["1LE1003-0DA22-2GC6","SIMOTICS GP MOTOR TYPE: 1AV3082A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 80M * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF165 (A200) 2 PTC thermistors for warning and shutdown (4 terminals) Terminal box lateral left",372,"ST",1,"LVM",11,1,"1LE10030DA222GC6"]
["1LE1003-0DA23-4GB5","SIMOTICS GP MOTOR TYPE: 1AV3082A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 80M * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF165 (A200) MOTOR PROTECTION WITH 1 PTC THERMISTORS FOR SHUTDOWN Terminal box lateral right",313,"ST",1,"LVM",11,1,"1LE10030DA234GB5"]
["1LE1003-0DA33-3FB5","SIMOTICS GP MOTOR TYPE: 1AV3083A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 80M * 1.1kW (50 Hz) 1.27kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 5, flange: FF165 (A200) MOTOR PROTECTION WITH 1 PTC THERMISTORS FOR SHUTDOWN Terminal box lateral right",366,"ST",1,"LVM",12,1,"1LE10030DA333FB5"]
["1LE1003-0DA33-4GA5","SIMOTICS GP MOTOR TYPE: 1AV3083A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 80M * 1.1kW (50 Hz) 1.27kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF165 (A200) WITHOUT MOTOR PROTECTION Terminal box lateral right",336,"ST",1,"LVM",12,1,"1LE10030DA334GA5"]
["1LE1003-0DB22-2AC5","SIMOTICS GP MOTOR TYPE: 1AV3082B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing Premium Efficiency, 4-pole * Size 80M * 0.55kW (50 Hz) 0.63kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 2 PTC thermistors for warning and shutdown (4 terminals) Terminal box lateral right",346,"ST",1,"LVM",11,1,"1LE10030DB222AC5"]
["1LE1003-0DB23-4JB6","SIMOTICS GP MOTOR TYPE: 1AV3082B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing Premium Efficiency, 4-pole * Size 80M * 0.55kW (50 Hz) 0.63kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF165 (A200) MOTOR PROTECTION WITH 1 PTC THERMISTORS FOR SHUTDOWN Terminal box lateral left",312,"ST",1,"LVM",11,1,"1LE10030DB234JB6"]
["1LE1003-0DB32-2AB5","SIMOTICS GP MOTOR TYPE: 1AV3083B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 80M * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, MOTOR PROTECTION WITH 1 PTC THERMISTORS FOR SHUTDOWN Terminal box lateral right",311,"ST",1,"LVM",14,1,"1LE10030DB322AB5"]
["1LE1003-0DC22-2GB4","SIMOTICS GP MOTOR TYPE: 1AV3082C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing Premium Efficiency, 6-pole * Size 80M * 0.37kW (50 Hz) 0.43kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF165 (A200) 1 PTC thermistor for disconnection (2 terminals) Terminal box at top",289,"ST",1,"LVM",12,1,"1LE10030DC222GB4"]
["1LE1003-0DC22-2JA5","SIMOTICS GP MOTOR TYPE: 1AV3082C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing Premium Efficiency, 6-pole * Size 80M * 0.37kW (50 Hz) 0.43kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF165 (A200) without motor protection Terminal box lateral right",289,"ST",1,"LVM",12,1,"1LE10030DC222JA5"]
["1LE1003-0DC33-4AA4","SIMOTICS GP MOTOR TYPE: 1AV3083C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing Premium Efficiency, 6-pole * Size 80M * 0.55kW (50 Hz) 0.63kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box at top",289,"ST",1,"LVM",14,1,"1LE10030DC334AA4"]
["1LE1003-0EA00-4FA4","SIMOTICS GP MOTOR TYPE: 1AV3090A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 90S * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF165 (A200) WITHOUT MOTOR PROTECTION Terminal box at top",371,"ST",1,"LVM",15,1,"1LE10030EA004FA4"]
["1LE1003-0EA03-4FB5","SIMOTICS GP MOTOR TYPE: 1AV3090A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 90S * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF165 (A200) MOTOR PROTECTION WITH 1 PTC THERMISTORS FOR SHUTDOWN Terminal box lateral right",406,"ST",1,"LVM",15,1,"1LE10030EA034FB5"]
["1LE1003-0EA42-1GB4","SIMOTICS GP MOTOR TYPE: 1AV3094A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 90L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF165 (A200) MOTOR PROTECTION WITH 1 PTC THERMISTORS FOR SHUTDOWN Terminal box at top",505,"ST",1,"LVM",19,1,"1LE10030EA421GB4"]
["1LE1003-0EB00-4FA5","SIMOTICS GP MOTOR TYPE: 1AV3090B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 90S * 1.1kW (50 Hz) 1.27kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF165 (A200) WITHOUT MOTOR PROTECTION Terminal box lateral right",378,"ST",1,"LVM",16,1,"1LE10030EB004FA5"]
["1LE1003-0EB02-2JC6","SIMOTICS GP MOTOR TYPE: 1AV3090B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 90S * 1.1kW (50 Hz) 1.27kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF165 (A200) 2 PTC thermistors for warning and shutdown (4 terminals) Terminal box lateral left",453,"ST",1,"LVM",16,1,"1LE10030EB022JC6"]
["1LE1003-0EB42-1GB6","SIMOTICS GP MOTOR TYPE: 1AV3094B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 90L * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF165 (A200) MOTOR PROTECTION WITH 1 PTC THERMISTORS FOR SHUTDOWN Terminal box lateral left",475,"ST",1,"LVM",19,1,"1LE10030EB421GB6"]
["1LE1003-0EB40-4FA4","SIMOTICS GP MOTOR TYPE: 1AV3094B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 90L * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF165 (A200) WITHOUT MOTOR PROTECTION Terminal box at top",422,"ST",1,"LVM",19,1,"1LE10030EB404FA4"]
["1LE1003-0EC02-2AB6","SIMOTICS GP MOTOR TYPE: 1AV3090C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 6-pole * Size 90S * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 1 PTC thermistor for disconnection (2 terminals) Terminal box lateral left",361,"ST",1,"LVM",16.001000000000001,1,"1LE10030EC022AB6"]
["1LE1003-0EC03-3GB5","SIMOTICS GP MOTOR TYPE: 1AV3090C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 6-pole * Size 90S * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF165 (A200) 1 PTC thermistor for disconnection (2 terminals) Terminal box lateral right",407,"ST",1,"LVM",16.001000000000001,1,"1LE10030EC033GB5"]
["1LE1003-0EC40-4JB6","SIMOTICS GP MOTOR TYPE: 1AV3094C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE1 6-pole * Size 90L * 1.1kW (50 Hz) 1.27kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF165 (A200) 1 PTC thermistor for disconnection (2 terminals) Terminal box lateral left",468,"ST",1,"LVM",19.001000000000001,1,"1LE10030EC404JB6"]
["1LE1003-0EC43-4AB5","SIMOTICS GP MOTOR TYPE: 1AV3094C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE1 6-pole * Size 90L * 1.1kW (50 Hz) 1.27kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 1 PTC thermistor for disconnection (2 terminals) Terminal box lateral right",439,"ST",1,"LVM",19.001000000000001,1,"1LE10030EC434AB5"]
["1LE1003-1AA42-2GA4","SIMOTICS GP MOTOR TYPE: 1AV3104A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF215 (A250) Without motor protection Terminal box at top",530,"ST",1,"LVM",26,1,"1LE10031AA422GA4"]
["1LE1003-1AA43-3AB5","SIMOTICS GP MOTOR TYPE: 1AV3104A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",612,"ST",1,"LVM",26,1,"1LE10031AA433AB5"]
["1LE1003-1AA43-3GA7","SIMOTICS GP MOTOR TYPE: 1AV3104A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF215 (A250) Without motor protection Terminal box below",597,"ST",1,"LVM",26,1,"1LE10031AA433GA7"]
["1LE1003-1AB42-2JC6","SIMOTICS GP MOTOR TYPE: 1AV3104B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 100L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF215 (A250) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",621,"ST",1,"LVM",30,1,"1LE10031AB422JC6"]
["1LE1003-1AB43-4JB5","SIMOTICS GP MOTOR TYPE: 1AV3104B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 100L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",585,"ST",1,"LVM",30,1,"1LE10031AB434JB5"]
["1LE1003-1AB52-2FA7","SIMOTICS GP MOTOR TYPE: 1AV3105B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF215 (A250) Without motor protection Terminal box below",603,"ST",1,"LVM",30,1,"1LE10031AB522FA7"]
["1LE1003-1AB53-4AB5","SIMOTICS GP MOTOR TYPE: 1AV3105B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",619,"ST",1,"LVM",30,1,"1LE10031AB534AB5"]
["1LE1003-1AC42-2AB5","SIMOTICS GP MOTOR TYPE: 1AV3104C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 100L * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",544,"ST",1,"LVM",25,1,"1LE10031AC422AB5"]
["1LE1003-1AC42-2GB7","SIMOTICS GP MOTOR TYPE: 1AV3104C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 100L * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",578,"ST",1,"LVM",25,1,"1LE10031AC422GB7"]
["1LE1003-1AC43-3JA5","SIMOTICS GP MOTOR TYPE: 1AV3104C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 100L * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 35, Flange: FF215 (A250) without motor protection Terminal box on RHS",554,"ST",1,"LVM",25,1,"1LE10031AC433JA5"]
["1LE1003-1BA22-2AC7","SIMOTICS GP MOTOR TYPE: 1AV3112A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",722,"ST",1,"LVM",34,1,"1LE10031BA222AC7"]
["1LE1003-1BB20-4JB4","SIMOTICS GP MOTOR TYPE: 1AV3112B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",735,"ST",1,"LVM",34,1,"1LE10031BB204JB4"]
["1LE1003-1BB22-1FA6","SIMOTICS GP MOTOR TYPE: 1AV3112B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF215 (A250) Without motor protection Terminal box on left-hand side",756,"ST",1,"LVM",34,1,"1LE10031BB221FA6"]
["1LE1003-1BB23-4JB6","SIMOTICS GP MOTOR TYPE: 1AV3112B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",783,"ST",1,"LVM",34,1,"1LE10031BB234JB6"]
["1LE1003-1BC22-1JA7","SIMOTICS GP MOTOR TYPE: 1AV3112C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 112M, * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35, Flange: FF215 (A250) without motor protection Terminal box below",693,"ST",1,"LVM",34,1,"1LE10031BC221JA7"]
["1LE1003-1BC23-4AC6","SIMOTICS GP MOTOR TYPE: 1AV3112C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 112M, * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",705,"ST",1,"LVM",34,1,"1LE10031BC234AC6"]
["1LE1003-1BC23-4JC6","SIMOTICS GP MOTOR TYPE: 1AV3112C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 112M, * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35, Flange: FF215 (A250) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",751,"ST",1,"LVM",34,1,"1LE10031BC234JC6"]
["1LE1003-1CA02-2GC7","SIMOTICS GP MOTOR TYPE: 1AV3130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",958,"ST",1,"LVM",43,1,"1LE10031CA022GC7"]
["1LE1003-1CA03-4AC7","SIMOTICS GP MOTOR TYPE: 1AV3130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",902,"ST",1,"LVM",43,1,"1LE10031CA034AC7"]
["1LE1003-1CA10-4FA4","SIMOTICS GP MOTOR TYPE: 1AV3131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF265 (A300) Without motor protection Terminal box at top",993,"ST",1,"LVM",57,1,"1LE10031CA104FA4"]
["1LE1003-1CA12-2WB7","SIMOTICS GP MOTOR TYPE: 1AV3131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 15 * Flange: FF265 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1134,"ST",1,"LVM",57,1,"1LE10031CA122WB7"]
["1LE1003-1CA13-3JB4","SIMOTICS GP MOTOR TYPE: 1AV3131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 35, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1105,"ST",1,"LVM",57,1,"1LE10031CA133JB4"]
["1LE1003-1CB02-2AA7","SIMOTICS GP MOTOR TYPE: 1AV3130B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 Without motor protection Terminal box below",854,"ST",1,"LVM",64,1,"1LE10031CB022AA7"]
["1LE1003-1CB02-2WC4","SIMOTICS GP MOTOR TYPE: 1AV3130B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 15 * Flange: FF265 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",987,"ST",1,"LVM",64,1,"1LE10031CB022WC4"]
["1LE1003-1CB20-4AB6","SIMOTICS GP MOTOR TYPE: 1AV3132B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 132M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1144,"ST",1,"LVM",64,1,"1LE10031CB204AB6"]
["1LE1003-1CB22-1WB7","SIMOTICS GP MOTOR TYPE: 1AV3132B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 132M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 15 * Flange: FF265 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1249,"ST",1,"LVM",64,1,"1LE10031CB221WB7"]
["1LE1003-1CB23-4FC4","SIMOTICS GP MOTOR TYPE: 1AV3132B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 132M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",1187,"ST",1,"LVM",64,1,"1LE10031CB234FC4"]
["1LE1003-1CC00-4JB4","SIMOTICS GP MOTOR TYPE: 1AV3130C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 132S, * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35, Flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",843,"ST",1,"LVM",43,1,"1LE10031CC004JB4"]
["1LE1003-1CC02-1FA5","SIMOTICS GP MOTOR TYPE: 1AV3130C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 132S, * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF265 (A300) without motor protection Terminal box on RHS",853,"ST",1,"LVM",43,1,"1LE10031CC021FA5"]
["1LE1003-1CC03-3AA6","SIMOTICS GP MOTOR TYPE: 1AV3130C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 132S, * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B3 without motor protection Terminal box on left-hand side",797,"ST",1,"LVM",43,1,"1LE10031CC033AA6"]
["1LE1003-1CC22-1FA4","SIMOTICS GP MOTOR TYPE: 1AV3132C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 132M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF265 (A300) without motor protection Terminal box at top",969,"ST",1,"LVM",52,1,"1LE10031CC221FA4"]
["1LE1003-1CC22-2GA6","SIMOTICS GP MOTOR TYPE: 1AV3132C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 132M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF265 (A300) without motor protection Terminal box on left-hand side",985,"ST",1,"LVM",52,1,"1LE10031CC222GA6"]
["1LE1003-1CC23-3FA7","SIMOTICS GP MOTOR TYPE: 1AV3132C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 132M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 5, flange: FF265 (A300) without motor protection Terminal box below",1021,"ST",1,"LVM",52,1,"1LE10031CC233FA7"]
["1LE1003-1CC23-4FA6","SIMOTICS GP MOTOR TYPE: 1AV3132C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 132M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF265 (A300) without motor protection Terminal box on left-hand side",985,"ST",1,"LVM",52,1,"1LE10031CC234FA6"]
["1LE1003-1CC33-3GB6","SIMOTICS GP MOTOR TYPE: 1AV3133C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 132M, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1323,"ST",1,"LVM",64,1,"1LE10031CC333GB6"]
["1LE1003-1CC33-4WB6","SIMOTICS GP MOTOR TYPE: 1AV3133C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 132M, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF265 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1302,"ST",1,"LVM",64,1,"1LE10031CC334WB6"]
["1LE1003-1CD02-1AA7","SIMOTICS GP MOTOR TYPE: 1AV3130D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 132S, * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B3 without motor protection Terminal box below",1184,"ST",1,"LVM",56,1,"1LE10031CD021AA7"]
["1LE1003-1CD03-4JA6","SIMOTICS GP MOTOR TYPE: 1AV3130D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 132S, * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35, Flange: FF265 (A300) without motor protection Terminal box on left-hand side",1206,"ST",1,"LVM",56,1,"1LE10031CD034JA6"]
["1LE1003-1CD22-2GC4","SIMOTICS GP MOTOR TYPE: 1AV3132D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 132M, * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",1486,"ST",1,"LVM",65,1,"1LE10031CD222GC4"]
["1LE1003-1DA20-4FB5","SIMOTICS GP MOTOR TYPE: 1AV3162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",1505,"ST",1,"LVM",75,1,"1LE10031DA204FB5"]
["1LE1003-1DA22-2AA6","SIMOTICS GP MOTOR TYPE: 1AV3162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 Without motor protection Terminal box on left-hand side",1358,"ST",1,"LVM",75,1,"1LE10031DA222AA6"]
["1LE1003-1DA23-4FA7","SIMOTICS GP MOTOR TYPE: 1AV3162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF300 (A350) Without motor protection Terminal box below",1429,"ST",1,"LVM",75,1,"1LE10031DA234FA7"]
["1LE1003-1DA30-4AB4","SIMOTICS GP MOTOR TYPE: 1AV3163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1781,"ST",1,"LVM",84,1,"1LE10031DA304AB4"]
["1LE1003-1DA32-2WC6","SIMOTICS GP MOTOR TYPE: 1AV3163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 15 * Flange: FF300 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",1977,"ST",1,"LVM",84,1,"1LE10031DA322WC6"]
["1LE1003-1DA33-3FA5","SIMOTICS GP MOTOR TYPE: 1AV3163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 5, flange: FF300 (A350) Without motor protection Terminal box on RHS",1876,"ST",1,"LVM",84,1,"1LE10031DA333FA5"]
["1LE1003-1DA42-1GA7","SIMOTICS GP MOTOR TYPE: 1AV3164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF300 (A350) Without motor protection Terminal box below",2199,"ST",1,"LVM",94,1,"1LE10031DA421GA7"]
["1LE1003-1DA42-2JA6","SIMOTICS GP MOTOR TYPE: 1AV3164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35, flange: FF300 (A350) Without motor protection Terminal box on left-hand side",2164,"ST",1,"LVM",94,1,"1LE10031DA422JA6"]
["1LE1003-1DB20-4AB5","SIMOTICS GP MOTOR TYPE: 1AV3162B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",1463,"ST",1,"LVM",83,1,"1LE10031DB204AB5"]
["1LE1003-1DB22-1JB5","SIMOTICS GP MOTOR TYPE: 1AV3162B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",1586,"ST",1,"LVM",83,1,"1LE10031DB221JB5"]
["1LE1003-1DB23-3FA5","SIMOTICS GP MOTOR TYPE: 1AV3162B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 5, flange: FF300 (A350) Without motor protection Terminal box on RHS",1502,"ST",1,"LVM",83,1,"1LE10031DB233FA5"]
["1LE1003-1DB23-4WB7","SIMOTICS GP MOTOR TYPE: 1AV3162B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF300 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1564,"ST",1,"LVM",83,1,"1LE10031DB234WB7"]
["1LE1003-1DB42-1GB6","SIMOTICS GP MOTOR TYPE: 1AV3164B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 160L, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1977,"ST",1,"LVM",100,1,"1LE10031DB421GB6"]
["1LE1003-1DB43-4AA5","SIMOTICS GP MOTOR TYPE: 1AV3164B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 160L, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 Without motor protection Terminal box on RHS",1786,"ST",1,"LVM",100,1,"1LE10031DB434AA5"]
["1LE1003-1DC20-4AB4","SIMOTICS GP MOTOR TYPE: 1AV3162C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 160M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1479,"ST",1,"LVM",93,1,"1LE10031DC204AB4"]
["1LE1003-1DC23-3WB6","SIMOTICS GP MOTOR TYPE: 1AV3162C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 160M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 15 * Flange: FF300 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1678,"ST",1,"LVM",93,1,"1LE10031DC233WB6"]
["1LE1003-1DC23-3FA4","SIMOTICS GP MOTOR TYPE: 1AV3162C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 160M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",1518,"ST",1,"LVM",93,1,"1LE10031DC233FA4"]
["1LE1003-1DC42-2AC6","SIMOTICS GP MOTOR TYPE: 1AV3164C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 160L, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",2103,"ST",1,"LVM",115,1,"1LE10031DC422AC6"]
["1LE1003-1DC42-2JC5","SIMOTICS GP MOTOR TYPE: 1AV3164C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 160L, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35, Flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",2182,"ST",1,"LVM",115,1,"1LE10031DC422JC5"]
["1LE1003-1DD20-4JA6","SIMOTICS GP MOTOR TYPE: 1AV3162D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 160M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35, Flange: FF300 (A350) without motor protection Terminal box on left-hand side",1757,"ST",1,"LVM",72,1,"1LE10031DD204JA6"]
["1LE1003-1DD23-3AA4","SIMOTICS GP MOTOR TYPE: 1AV3162D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 160M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B3 without motor protection Terminal box at top",1665,"ST",1,"LVM",72,1,"1LE10031DD233AA4"]
["1LE1003-1DD32-1AA4","SIMOTICS GP MOTOR TYPE: 1AV3163D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 160M, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B3 without motor protection Terminal box at top",1997,"ST",1,"LVM",86,1,"1LE10031DD321AA4"]
["1LE1003-1DD32-2JC5","SIMOTICS GP MOTOR TYPE: 1AV3163D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 160M, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35, Flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",2203,"ST",1,"LVM",86,1,"1LE10031DD322JC5"]
["1LE1003-1DD42-2AA4","SIMOTICS GP MOTOR TYPE: 1AV3164D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 160L, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 without motor protection Terminal box at top",2323,"ST",1,"LVM",110,1,"1LE10031DD422AA4"]
["1LE1003-1DD43-3AA6","SIMOTICS GP MOTOR TYPE: 1AV3164D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 160L, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B3 without motor protection Terminal box on left-hand side",2422,"ST",1,"LVM",110,1,"1LE10031DD433AA6"]
["1LE1003-1DD43-4JA7","SIMOTICS GP MOTOR TYPE: 1AV3164D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 160L, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35, Flange: FF300 (A350) without motor protection Terminal box below",2458,"ST",1,"LVM",110,1,"1LE10031DD434JA7"]
["1LE1003-1EB22-1JA5","SIMOTICS GP MOTOR TYPE: 1AV3182B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 180 * 18.5kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box on RHS",2193,"ST",1,"LVM",134,1,"1LE10031EB221JA5"]
["1LE1003-1EB22-2JB4","SIMOTICS GP MOTOR TYPE: 1AV3182B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 180 * 18.5kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2132,"ST",1,"LVM",134,1,"1LE10031EB222JB4"]
["1LE1003-1EB42-2JA6","SIMOTICS GP MOTOR TYPE: 1AV3184B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 180 * 22kW (50 Hz) 25.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box on left-hand side",2433,"ST",1,"LVM",142,1,"1LE10031EB422JA6"]
["1LE1003-1EB43-4GA5","SIMOTICS GP MOTOR TYPE: 1AV3184B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 180 * 22kW (50 Hz) 25.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) without motor protection Terminal box on RHS",2413,"ST",1,"LVM",142,1,"1LE10031EB434GA5"]
["1LE1003-1ED40-4GB6","SIMOTICS GP MOTOR TYPE: 1AV3184D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 180 * 11kW (50 Hz) 13.2kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",3110,"ST",1,"LVM",161,1,"1LE10031ED404GB6"]
["1LE1003-1ED42-2AA4","SIMOTICS GP MOTOR TYPE: 1AV3184D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 180 * 11kW (50 Hz) 13.2kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, without motor protection Terminal box at top",2819,"ST",1,"LVM",161,1,"1LE10031ED422AA4"]
["1LE1003-2AA42-2GC6","SIMOTICS GP MOTOR TYPE: 1AV3204A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 200 * 30kW (50 Hz) 33.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF350 (A400) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",3345,"ST",1,"LVM",173,1,"1LE10032AA422GC6"]
["1LE1003-2AA43-4JB5","SIMOTICS GP MOTOR TYPE: 1AV3204A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 200 * 30kW (50 Hz) 33.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",3309,"ST",1,"LVM",173,1,"1LE10032AA434JB5"]
["1LE1003-2AB52-1GB4","SIMOTICS GP MOTOR TYPE: 1AV3205B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 200 * 30kW (50 Hz) 34.5kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",3193,"ST",1,"LVM",189,1,"1LE10032AB521GB4"]
["1LE1003-2AB53-4AA5","SIMOTICS GP MOTOR TYPE: 1AV3205B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 200 * 30kW (50 Hz) 34.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 without motor protection Terminal box on RHS",2990,"ST",1,"LVM",189,1,"1LE10032AB534AA5"]
["1LE1003-2AC43-4GA4","SIMOTICS GP MOTOR TYPE: 1AV3204C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 200 * 18.5kW (50 Hz) 22 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF350 (A400) without motor protection Terminal box at top",3047,"ST",1,"LVM",166,1,"1LE10032AC434GA4"]
["1LE1003-2AD52-1AA6","SIMOTICS GP MOTOR TYPE: 1AV3205D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 200 * 15kW (50 Hz) 18kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, without motor protection Terminal box on left-hand side",3846,"ST",1,"LVM",212,1,"1LE10032AD521AA6"]
["1LE1004-1AA42-1FA4","SIMOTICS GP MOTOR TYPE: 1AV4104A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF215 (A250) without motor protection Terminal box at top",658,"ST",1,"LVM",27,1,"1LE10041AA421FA4"]
["1LE1004-1AA42-2AC5","SIMOTICS GP MOTOR TYPE: 1AV4104A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",731,"ST",1,"LVM",27,1,"1LE10041AA422AC5"]
["1LE1004-1AA43-4JB4","SIMOTICS GP MOTOR TYPE: 1AV4104A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",689,"ST",1,"LVM",27,1,"1LE10041AA434JB4"]
["1LE1004-1AB42-1AA6","SIMOTICS GP MOTOR TYPE: 1AV4104B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 100L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, without motor protection Terminal box on left-hand side",621,"ST",1,"LVM",30,1,"1LE10041AB421AA6"]
["1LE1004-1AB43-4FA7","SIMOTICS GP MOTOR TYPE: 1AV4104B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 100L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF215 (A250) without motor protection Terminal box below",633,"ST",1,"LVM",30,1,"1LE10041AB434FA7"]
["1LE1004-1AB50-4GB6","SIMOTICS GP MOTOR TYPE: 1AV4105B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",762,"ST",1,"LVM",38,1,"1LE10041AB504GB6"]
["1LE1004-1AB52-1GB7","SIMOTICS GP MOTOR TYPE: 1AV4105B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",785,"ST",1,"LVM",38,1,"1LE10041AB521GB7"]
["1LE1004-1AB53-4FC7","SIMOTICS GP MOTOR TYPE: 1AV4105B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF215 (A250) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",799,"ST",1,"LVM",38,1,"1LE10041AB534FC7"]
["1LE1004-1BA20-4JB4","SIMOTICS GP MOTOR TYPE: 1AV4112A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",806,"ST",1,"LVM",34,1,"1LE10041BA204JB4"]
["1LE1004-1BA23-4AC5","SIMOTICS GP MOTOR TYPE: 1AV4112A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",844,"ST",1,"LVM",34,1,"1LE10041BA234AC5"]
["1LE1004-1BB20-4AB5","SIMOTICS GP MOTOR TYPE: 1AV4112B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",875,"ST",1,"LVM",46,1,"1LE10041BB204AB5"]
["1LE1004-1BB23-3AA7","SIMOTICS GP MOTOR TYPE: 1AV4112B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 3, without motor protection Terminal box below",852,"ST",1,"LVM",46,1,"1LE10041BB233AA7"]
["1LE1004-1BB23-4AB6","SIMOTICS GP MOTOR TYPE: 1AV4112B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",875,"ST",1,"LVM",46,1,"1LE10041BB234AB6"]
["1LE1004-1CA02-2FC6","SIMOTICS GP MOTOR TYPE: 1AV4130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",1117,"ST",1,"LVM",44,1,"1LE10041CA022FC6"]
["1LE1004-1CA02-2GA4","SIMOTICS GP MOTOR TYPE: 1AV4130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF265 (A300) without motor protection Terminal box at top",951,"ST",1,"LVM",44,1,"1LE10041CA022GA4"]
["1LE1004-1CA10-4FB6","SIMOTICS GP MOTOR TYPE: 1AV4131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1317,"ST",1,"LVM",56,1,"1LE10041CA104FB6"]
["1LE1004-1CA12-2AA4","SIMOTICS GP MOTOR TYPE: 1AV4131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, without motor protection Terminal box at top",1134,"ST",1,"LVM",56,1,"1LE10041CA122AA4"]
["1LE1004-1CA13-4FC7","SIMOTICS GP MOTOR TYPE: 1AV4131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",1357,"ST",1,"LVM",56,1,"1LE10041CA134FC7"]
["1LE1004-1CB00-4FB7","SIMOTICS GP MOTOR TYPE: 1AV4130B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1153,"ST",1,"LVM",59,1,"1LE10041CB004FB7"]
["1LE1004-1CB02-2GC4","SIMOTICS GP MOTOR TYPE: 1AV4130B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",1141,"ST",1,"LVM",59,1,"1LE10041CB022GC4"]
["1LE1004-1CB03-3WB4","SIMOTICS GP MOTOR TYPE: 1AV4130B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 15 * Flange: FF265 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1151,"ST",1,"LVM",59,1,"1LE10041CB033WB4"]
["1LE1004-1CB03-4WB7","SIMOTICS GP MOTOR TYPE: 1AV4130B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF265 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1168,"ST",1,"LVM",59,1,"1LE10041CB034WB7"]
["1LE1004-1CB22-2JA5","SIMOTICS GP MOTOR TYPE: 1AV4132B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 132M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF265 (A300) without motor protection Terminal box on RHS",1336,"ST",1,"LVM",62,1,"1LE10041CB222JA5"]
["1LE1004-1CB23-3WB6","SIMOTICS GP MOTOR TYPE: 1AV4132B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 132M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 15 * Flange: FF265 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1459,"ST",1,"LVM",62,1,"1LE10041CB233WB6"]
["1LE1004-1DA20-4GA5","SIMOTICS GP MOTOR TYPE: 1AV4162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) without motor protection Terminal box on RHS",1707,"ST",1,"LVM",84,1,"1LE10041DA204GA5"]
["1LE1004-1DA22-2FB7","SIMOTICS GP MOTOR TYPE: 1AV4162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1782,"ST",1,"LVM",84,1,"1LE10041DA222FB7"]
["1LE1004-1DA30-4AA4","SIMOTICS GP MOTOR TYPE: 1AV4163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box at top",2058,"ST",1,"LVM",98,1,"1LE10041DA304AA4"]
["1LE1004-1DA30-4WB5","SIMOTICS GP MOTOR TYPE: 1AV4163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF300 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",2290,"ST",1,"LVM",98,1,"1LE10041DA304WB5"]
["1LE1004-1DA32-2AA4","SIMOTICS GP MOTOR TYPE: 1AV4163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, without motor protection Terminal box at top",2058,"ST",1,"LVM",98,1,"1LE10041DA322AA4"]
["1LE1004-1DA33-4JA4","SIMOTICS GP MOTOR TYPE: 1AV4163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2138,"ST",1,"LVM",98,1,"1LE10041DA334JA4"]
["1LE1004-1DA42-2FB5","SIMOTICS GP MOTOR TYPE: 1AV4164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",2660,"ST",1,"LVM",112,1,"1LE10041DA422FB5"]
["1LE1004-1DA43-3GA6","SIMOTICS GP MOTOR TYPE: 1AV4164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF300 (A350) without motor protection Terminal box on left-hand side",2628,"ST",1,"LVM",112,1,"1LE10041DA433GA6"]
["1LE1004-1DB22-1AA4","SIMOTICS GP MOTOR TYPE: 1AV4162B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, without motor protection Terminal box at top",1657,"ST",1,"LVM",98,1,"1LE10041DB221AA4"]
["1LE1004-1DB22-2AC5","SIMOTICS GP MOTOR TYPE: 1AV4162B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",1784,"ST",1,"LVM",98,1,"1LE10041DB222AC5"]
["1LE1004-1DB23-3FA5","SIMOTICS GP MOTOR TYPE: 1AV4162B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 5, flange: FF300 (A350) without motor protection Terminal box on RHS",1783,"ST",1,"LVM",98,1,"1LE10041DB233FA5"]
["1LE1004-1DB23-4JC4","SIMOTICS GP MOTOR TYPE: 1AV4162B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",1808,"ST",1,"LVM",98,1,"1LE10041DB234JC4"]
["1LE1004-1DB42-2WC7","SIMOTICS GP MOTOR TYPE: 1AV4164B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 160L, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 15 * Flange: FF300 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",2359,"ST",1,"LVM",109,1,"1LE10041DB422WC7"]
["1LE1004-1DB43-4FB6","SIMOTICS GP MOTOR TYPE: 1AV4164B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 160L, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",2290,"ST",1,"LVM",109,1,"1LE10041DB434FB6"]
["1LE1023-0DB39-0FA4","SIMOTICS GP MOTOR TYPE: 1AV3083B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing IE3, NEMA Premium, CSA, UL, 4-pole * Size 80M * 0.75kW (50 Hz) NEMA 60Hz: 1HP 3 AC 60 Hz 575 VD * 50 Hz power IM B 5, flange: FF165 (A200) without motor protection Terminal box at top",361,"ST",1,"LVM",14,1,"1LE10230DB390FA4"]
["1LE1023-1CB29-0GA4","SIMOTICS GP MOTOR TYPE: 1AV3132B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing IE3, NEMA Premium, CSA, UL, 4-pole * Size 132M, * 7.5kW (50 Hz) NEMA 60Hz: 10HP 3 AC 60 Hz 460 VD * 50 Hz power IM V 1 without canopy, flange: FF265 (A300) without motor protection Terminal box at top",1229,"ST",1,"LVM",64,1,"1LE10231CB290GA4"]
["1LE1501-0CA22-2JC4","SIMOTICS SD MOTOR TYPE: 1CV2072A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 2-pole * Size 71M * 0.37kW (50 Hz) 0.43kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF130 (A160) 2 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",317,"ST",1,"LVM",11.5,1,"1LE15010CA222JC4"]
["1LE1501-1CA03-4AA5","SIMOTICS SD MOTOR TYPE: 1CV2130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) High Efficiency IE2, 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box on RHS",762,"ST",1,"LVM",57,1,"1LE15011CA034AA5"]
["1LE1501-1CA12-2JC4","SIMOTICS SD MOTOR TYPE: 1CV2131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",1080,"ST",1,"LVM",61,1,"1LE15011CA122JC4"]
["1LE1501-1DA42-2JA6","SIMOTICS SD MOTOR TYPE: 1CV2164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations to be considered! 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box on left-hand side",2084,"ST",1,"LVM",113,1,"1LE15011DA422JA6"]
["1LE1501-1EA20-4FA5","SIMOTICS SD MOTOR TYPE: 1CV2182A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 180M, * 22kW (50 Hz) 24.5kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF300 (A350) without motor protection Terminal box on RHS",2453,"ST",1,"LVM",145,1,"1LE15011EA204FA5"]
["1LE1501-1EA22-2JB6","SIMOTICS SD MOTOR TYPE: 1CV2182A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 180M, * 22kW (50 Hz) 24.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",2573,"ST",1,"LVM",145,1,"1LE15011EA222JB6"]
["1LE1501-1EA23-3FB4","SIMOTICS SD MOTOR TYPE: 1CV2182A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 180M, * 22kW (50 Hz) 24.5kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2456,"ST",1,"LVM",145,1,"1LE15011EA233FB4"]
["1LE1501-1EB22-2WB5","SIMOTICS SD MOTOR TYPE: 1CV2182B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 180M, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 15 * Flange: FF300 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",2261,"ST",1,"LVM",160,1,"1LE15011EB222WB5"]
["1LE1501-1EB23-4AB6","SIMOTICS SD MOTOR TYPE: 1CV2182B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 180M, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",2109,"ST",1,"LVM",160,1,"1LE15011EB234AB6"]
["1LE1501-1EB42-2FB5","SIMOTICS SD MOTOR TYPE: 1CV2184B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 180L, * 22kW (50 Hz) 25.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",2524,"ST",1,"LVM",170,1,"1LE15011EB422FB5"]
["1LE1501-1EB43-4FC4","SIMOTICS SD MOTOR TYPE: 1CV2184B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 180L, * 22kW (50 Hz) 25.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",2445,"ST",1,"LVM",170,1,"1LE15011EB434FC4"]
["1LE1501-1EC42-2AC6","SIMOTICS SD MOTOR TYPE: 1CV2184C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 6-pole * Size 180L, * 15kW (50 Hz) 18kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",2631,"ST",1,"LVM",155,1,"1LE15011EC422AC6"]
["1LE1501-1EC43-4AA6","SIMOTICS SD MOTOR TYPE: 1CV2184C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 6-pole * Size 180L, * 15kW (50 Hz) 18kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box on left-hand side",2454,"ST",1,"LVM",155,1,"1LE15011EC434AA6"]
["1LE1501-1EC43-4WB5","SIMOTICS SD MOTOR TYPE: 1CV2184C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 6-pole * Size 180L, * 15kW (50 Hz) 18kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF300 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",2707,"ST",1,"LVM",155,1,"1LE15011EC434WB5"]
["1LE1501-2AA43-3GA6","SIMOTICS SD MOTOR TYPE: 1CV2204A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 200L, * 30kW (50 Hz) 33.5kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF350 (A400) without motor protection Terminal box on left-hand side",3218,"ST",1,"LVM",200,1,"1LE15012AA433GA6"]
["1LE1501-2AA50-4FB6","SIMOTICS SD MOTOR TYPE: 1CV2205A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 200L, * 37kW (50 Hz) 41.5kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",3975,"ST",1,"LVM",225,1,"1LE15012AA504FB6"]
["1LE1501-2AA53-4GB5","SIMOTICS SD MOTOR TYPE: 1CV2205A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 200L, * 37kW (50 Hz) 41.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",3974,"ST",1,"LVM",225,1,"1LE15012AA534GB5"]
["1LE1501-2AB52-2GB6","SIMOTICS SD MOTOR TYPE: 1CV2205B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 200L, * 30kW (50 Hz) 34.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",3209,"ST",1,"LVM",230,1,"1LE15012AB522GB6"]
["1LE1501-2AB53-3JA4","SIMOTICS SD MOTOR TYPE: 1CV2205B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 200L, * 30kW (50 Hz) 34.5kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF350 (A400) without motor protection Terminal box at top",3032,"ST",1,"LVM",230,1,"1LE15012AB533JA4"]
["1LE1501-2AB53-4GC5","SIMOTICS SD MOTOR TYPE: 1CV2205B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 200L, * 30kW (50 Hz) 34.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF350 (A400) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",3286,"ST",1,"LVM",230,1,"1LE15012AB534GC5"]
["1LE1501-2AC43-4AA6","SIMOTICS SD MOTOR TYPE: 1CV2204C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 200L, * 18.5 kW (50 Hz) 22 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box on left-hand side",2990,"ST",1,"LVM",200,1,"1LE15012AC434AA6"]
["1LE1501-2AC50-4JA5","SIMOTICS SD MOTOR TYPE: 1CV2205C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 200L, * 22kW (50 Hz) 26.5kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF350 (A400) without motor protection Terminal box on RHS",3611,"ST",1,"LVM",220,1,"1LE15012AC504JA5"]
["1LE1501-2AC53-3AA5","SIMOTICS SD MOTOR TYPE: 1CV2205C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 200L, * 22kW (50 Hz) 26.5kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, without motor protection Terminal box on RHS",3502,"ST",1,"LVM",220,1,"1LE15012AC533AA5"]
["1LE1501-2AC53-4JB5","SIMOTICS SD MOTOR TYPE: 1CV2205C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 200L, * 22kW (50 Hz) 26.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",3712,"ST",1,"LVM",220,1,"1LE15012AC534JB5"]
["1LE1501-2BA23-3GA5","SIMOTICS SD MOTOR TYPE: 1CV2222A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 225M * 45kW (50 Hz) 51kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF400 (A450) without motor protection Terminal box on RHS",4585,"ST",1,"LVM",295,1,"1LE15012BA233GA5"]
["1LE1501-2BA23-4JB6","SIMOTICS SD MOTOR TYPE: 1CV2222A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 225M * 45kW (50 Hz) 51kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF400 (A450) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",4674,"ST",1,"LVM",295,1,"1LE15012BA234JB6"]
["1LE1501-2BB00-4AB5","SIMOTICS SD MOTOR TYPE: 1CV2220B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 225S * 37kW (50 Hz) 42.5kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",3626,"ST",1,"LVM",280,1,"1LE15012BB004AB5"]
["1LE1501-2BB20-4JA6","SIMOTICS SD MOTOR TYPE: 1CV2222B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 225M * 45kW (50 Hz) 52kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF400 (A450) without motor protection Terminal box on left-hand side",4294,"ST",1,"LVM",305,1,"1LE15012BB204JA6"]
["1LE1501-2BB22-1FA4","SIMOTICS SD MOTOR TYPE: 1CV2222B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 225M * 45kW (50 Hz) 52kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF400 (A450) without motor protection Terminal box at top",4124,"ST",1,"LVM",305,1,"1LE15012BB221FA4"]
["1LE1501-2BB23-4GB6","SIMOTICS SD MOTOR TYPE: 1CV2222B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 225M * 45kW (50 Hz) 52kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF400 (A450) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",4388,"ST",1,"LVM",305,1,"1LE15012BB234GB6"]
["1LE1501-2BC23-3AA6","SIMOTICS SD MOTOR TYPE: 1CV2222C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 225M * 30kW (50 Hz) 36 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, without motor protection Terminal box on left-hand side",4508,"ST",1,"LVM",300,1,"1LE15012BC233AA6"]
["1LE1501-2BC23-4AC4","SIMOTICS SD MOTOR TYPE: 1CV2222C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 225M * 30kW (50 Hz) 36 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",4431,"ST",1,"LVM",300,1,"1LE15012BC234AC4"]
["1LE1501-2CA20-4JA6","SIMOTICS SD MOTOR TYPE: 1CV2252A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 250M * 55kW (50 Hz) 62kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF500 (A550) without motor protection Terminal box on left-hand side",5462,"ST",1,"LVM",360,1,"1LE15012CA204JA6"]
["1LE1501-2CA23-4FB5","SIMOTICS SD MOTOR TYPE: 1CV2252A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 250M * 55kW (50 Hz) 62kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",5502,"ST",1,"LVM",360,1,"1LE15012CA234FB5"]
["1LE1501-2CB20-4AB5","SIMOTICS SD MOTOR TYPE: 1CV2252B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 250M * 55kW (50 Hz) 63kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",5122,"ST",1,"LVM",385,1,"1LE15012CB204AB5"]
["1LE1501-2CB23-3GA5","SIMOTICS SD MOTOR TYPE: 1CV2252B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 250M * 55kW (50 Hz) 63kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF500 (A550) without motor protection Terminal box on RHS",5306,"ST",1,"LVM",385,1,"1LE15012CB233GA5"]
["1LE1501-2CC20-4AA6","SIMOTICS SD MOTOR TYPE: 1CV2252C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 250M * 37kW (50 Hz) 44.5kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box on left-hand side",5405,"ST",1,"LVM",370,1,"1LE15012CC204AA6"]
["1LE1501-2CC23-4FB6","SIMOTICS SD MOTOR TYPE: 1CV2252C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 250M * 37kW (50 Hz) 44.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",5754,"ST",1,"LVM",370,1,"1LE15012CC234FB6"]
["1LE1501-2DA02-1AA6","SIMOTICS SD MOTOR TYPE: 1CV2280A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 280S, * 75kW (50 Hz) 84kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, without motor protection Terminal box on left-hand side",7174,"ST",1,"LVM",490,1,"1LE15012DA021AA6"]
["1LE1501-2DA03-3WB5","SIMOTICS SD MOTOR TYPE: 1CV2280A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 280S, * 75kW (50 Hz) 84kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 15 * Flange: FF500 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",7870,"ST",1,"LVM",490,1,"1LE15012DA033WB5"]
["1LE1501-2DA03-4GC6","SIMOTICS SD MOTOR TYPE: 1CV2280A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 280S, * 75kW (50 Hz) 84kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF500 (A550) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",7638,"ST",1,"LVM",490,1,"1LE15012DA034GC6"]
["1LE1501-2DA23-4FC4","SIMOTICS SD MOTOR TYPE: 1CV2282A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 280M * 90kW (50 Hz) 101kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF500 (A550) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",8492,"ST",1,"LVM",530,1,"1LE15012DA234FC4"]
["1LE1501-2DB00-4AB5","SIMOTICS SD MOTOR TYPE: 1CV2280B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 280S, * 75kW (50 Hz) 86kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",6791,"ST",1,"LVM",550,1,"1LE15012DB004AB5"]
["1LE1501-2DB03-4GB5","SIMOTICS SD MOTOR TYPE: 1CV2280B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 280S, * 75kW (50 Hz) 86kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",7103,"ST",1,"LVM",550,1,"1LE15012DB034GB5"]
["1LE1501-2DB22-1GB4","SIMOTICS SD MOTOR TYPE: 1CV2282B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 280M * 90kW (50 Hz) 104kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",7966,"ST",1,"LVM",570,1,"1LE15012DB221GB4"]
["1LE1501-2DB22-2GB4","SIMOTICS SD MOTOR TYPE: 1CV2282B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 280M * 90kW (50 Hz) 104kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",7833,"ST",1,"LVM",570,1,"1LE15012DB222GB4"]
["1LE1501-2DC02-1GA6","SIMOTICS SD MOTOR TYPE: 1CV2280C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 280S, * 45kW (50 Hz) 54kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF500 (A550) without motor protection Terminal box on left-hand side",7024,"ST",1,"LVM",460,1,"1LE15012DC021GA6"]
["1LE1501-2DC02-2GA6","SIMOTICS SD MOTOR TYPE: 1CV2280C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 280S, * 45kW (50 Hz) 54kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF500 (A550) without motor protection Terminal box on left-hand side",6891,"ST",1,"LVM",460,1,"1LE15012DC022GA6"]
["1LE1501-2DC22-1GB5","SIMOTICS SD MOTOR TYPE: 1CV2282C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 280M * 55kW (50 Hz) 66kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",8328,"ST",1,"LVM",510,1,"1LE15012DC221GB5"]
["1LE1501-2DC22-2GC4","SIMOTICS SD MOTOR TYPE: 1CV2282C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 280M * 55kW (50 Hz) 66kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF500 (A550) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",7947,"ST",1,"LVM",510,1,"1LE15012DC222GC4"]
["1LE1501-3AA02-1FA5","SIMOTICS SD MOTOR TYPE: 1CV2310A low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 315S, * 110kW (50 Hz) 123kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, Flange: FF600 (A660) without motor protection Terminal box on RHS",10440,"ST",1,"LVM",720,1,"1LE15013AA021FA5"]
["1LE1501-3AA02-2AB6","SIMOTICS SD MOTOR TYPE: 1CV2310A low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 315S, * 110kW (50 Hz) 123kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",9996,"ST",1,"LVM",720,1,"1LE15013AA022AB6"]
["1LE1501-3AA22-2AB6","SIMOTICS SD MOTOR TYPE: 1CV2312A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 315M, * 132kW (50 Hz) 148kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",11928,"ST",1,"LVM",880,1,"1LE15013AA222AB6"]
["1LE1501-3AA23-3AB6","SIMOTICS SD MOTOR TYPE: 1CV2312A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 315M, * 132kW (50 Hz) 148kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",12101,"ST",1,"LVM",880,1,"1LE15013AA233AB6"]
["1LE1501-3AA43-4AA6","SIMOTICS SD MOTOR TYPE: 1CV2314A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 315L, * 160kW (50 Hz) 180kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box on left-hand side",14530,"ST",1,"LVM",930,1,"1LE15013AA434AA6"]
["1LE1501-3AA50-4GA6","SIMOTICS SD MOTOR TYPE: 1CV2315A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 315L, * 200kW (50 Hz) 224kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, Flange: FF600 (A660) without motor protection Terminal box on left-hand side",18604,"ST",1,"LVM",1130,1,"1LE15013AA504GA6"]
["1LE1501-3AB00-4FB5","SIMOTICS SD MOTOR TYPE: 1CV2310B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 315S, * 110kW (50 Hz) 127kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",10227,"ST",1,"LVM",740,1,"1LE15013AB004FB5"]
["1LE1501-3AB02-2GA4","SIMOTICS SD MOTOR TYPE: 1CV2310B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 315S, * 110kW (50 Hz) 127kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, Flange: FF600 (A660) without motor protection Terminal box at top",9644,"ST",1,"LVM",740,1,"1LE15013AB022GA4"]
["1LE1501-3AB20-4JA4","SIMOTICS SD MOTOR TYPE: 1CV2312B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 315M, * 132kW (50 Hz) 152kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF600 (A660) without motor protection Terminal box at top",11424,"ST",1,"LVM",870,1,"1LE15013AB204JA4"]
["1LE1501-3AB23-3AB5","SIMOTICS SD MOTOR TYPE: 1CV2312B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 315M, * 132kW (50 Hz) 152kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",11681,"ST",1,"LVM",870,1,"1LE15013AB233AB5"]
["1LE1501-3AB42-2JB5","SIMOTICS SD MOTOR TYPE: 1CV2314B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 315L, * 160kW (50 Hz) 184kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",14238,"ST",1,"LVM",940,1,"1LE15013AB422JB5"]
["1LE1501-3AB43-4GB4","SIMOTICS SD MOTOR TYPE: 1CV2314B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 315L, * 160kW (50 Hz) 184kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",13762,"ST",1,"LVM",940,1,"1LE15013AB434GB4"]
["1LE1501-3AB23-4JA6","SIMOTICS SD MOTOR TYPE: 1CV2312B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 315M, * 132kW (50 Hz) 152kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF600 (A660) without motor protection Terminal box on left-hand side",11842,"ST",1,"LVM",870,1,"1LE15013AB234JA6"]
["1LE1501-3AC00-4FA6","SIMOTICS SD MOTOR TYPE: 1CV2310C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 315S, * 75kW (50 Hz) 90 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, Flange: FF600 (A660) without motor protection Terminal box on left-hand side",10939,"ST",1,"LVM",660,1,"1LE15013AC004FA6"]
["1LE1501-3AC20-4FA6","SIMOTICS SD MOTOR TYPE: 1CV2312C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 315M, * 90kW (50 Hz) 108kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, Flange: FF600 (A660) without motor protection Terminal box on left-hand side",12199,"ST",1,"LVM",730,1,"1LE15013AC204FA6"]
["1LE1501-3AC22-2GA5","SIMOTICS SD MOTOR TYPE: 1CV2312C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 315M, * 90kW (50 Hz) 108kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, Flange: FF600 (A660) without motor protection Terminal box on RHS",12203,"ST",1,"LVM",730,1,"1LE15013AC222GA5"]
["1LE1501-3AC23-3GA4","SIMOTICS SD MOTOR TYPE: 1CV2312C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 315M, * 90kW (50 Hz) 108kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, Flange: FF600 (A660) without motor protection Terminal box at top",11959,"ST",1,"LVM",730,1,"1LE15013AC233GA4"]
["1LE1501-3AC43-4AC4","SIMOTICS SD MOTOR TYPE: 1CV2314C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 315L, * 110kW (50 Hz) 132 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",13894,"ST",1,"LVM",940,1,"1LE15013AC434AC4"]
["1LE1501-3AC50-4JA4","SIMOTICS SD MOTOR TYPE: 1CV2315C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations to be considered! 6-pole * Size 315L, * 132kW (50 Hz) 158kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF600 (A660) without motor protection Terminal box at top",16758,"ST",1,"LVM",990,1,"1LE15013AC504JA4"]
["1LE1501-3AC63-3GB4","SIMOTICS SD MOTOR TYPE: 1CV2316C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations to be considered! 6-pole * Size 315L, * 160kW (50 Hz) 192kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",20445,"ST",1,"LVM",1160,1,"1LE15013AC633GB4"]
["1LE1503-0CA23-4GA4","SIMOTICS SD MOTOR TYPE: 1CV3072A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 71M * 0.37kW (50 Hz) 0.43kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF130 (A160) without motor protection Terminal box at top",298,"ST",1,"LVM",13,1,"1LE15030CA234GA4"]
["1LE1503-0DA22-2GA5","SIMOTICS SD MOTOR TYPE: 1CV3082A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 80M * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF165 (A200) without motor protection Terminal box on RHS",380,"ST",1,"LVM",18,1,"1LE15030DA222GA5"]
["1LE1503-0DA23-4GA6","SIMOTICS SD MOTOR TYPE: 1CV3082A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 80M * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF165 (A200) without motor protection Terminal box on left-hand side",380,"ST",1,"LVM",18,1,"1LE15030DA234GA6"]
["1LE1503-0DA33-4GB6","SIMOTICS SD MOTOR TYPE: 1CV3083A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 80M * 1.1kW (50 Hz) 1.27kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF165 (A200) 1 PTC thermistor for disconnection (2 terminals) Terminal box on left-hand side",444,"ST",1,"LVM",21,1,"1LE15030DA334GB6"]
["1LE1503-0EA00-4AA5","SIMOTICS SD MOTOR TYPE: 1CV3090A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 90S * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box on RHS",472,"ST",1,"LVM",25.5,1,"1LE15030EA004AA5"]
["1LE1503-0EA03-4AC6","SIMOTICS SD MOTOR TYPE: 1CV3090A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 90S * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 2 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",546,"ST",1,"LVM",25.5,1,"1LE15030EA034AC6"]
["1LE1503-0EA43-4AA4","SIMOTICS SD MOTOR TYPE: 1CV3094A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 90L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box at top",542,"ST",1,"LVM",32,1,"1LE15030EA434AA4"]
["1LE1503-1AA43-3AB5","SIMOTICS SD MOTOR TYPE: 1CV3104A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",663,"ST",1,"LVM",36,1,"1LE15031AA433AB5"]
["1LE1503-1BA20-4GB4","SIMOTICS SD MOTOR TYPE: 1CV3112A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",735,"ST",1,"LVM",45,1,"1LE15031BA204GB4"]
["1LE1503-0EA43-4JC6","SIMOTICS SD MOTOR TYPE: 1CV3094A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 90L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF165 (A200) 2 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",676,"ST",1,"LVM",32,1,"1LE15030EA434JC6"]
["1LE1503-1CA00-4GA4","SIMOTICS SD MOTOR TYPE: 1CV3130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF265 (A300) without motor protection Terminal box at top",858,"ST",1,"LVM",58,1,"1LE15031CA004GA4"]
["1LE1503-1CA02-1JA5","SIMOTICS SD MOTOR TYPE: 1CV3130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF265 (A300) without motor protection Terminal box on RHS",947,"ST",1,"LVM",58,1,"1LE15031CA021JA5"]
["1LE1503-1CA10-4JA7","SIMOTICS SD MOTOR TYPE: 1CV3131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF265 (A300) without motor protection Terminal box below",1139,"ST",1,"LVM",73,1,"1LE15031CA104JA7"]
["1LE1503-1CA12-2AC6","SIMOTICS SD MOTOR TYPE: 1CV3131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",1196,"ST",1,"LVM",73,1,"1LE15031CA122AC6"]
["1LE1503-1DA22-2GB7","SIMOTICS SD MOTOR TYPE: 1CV3162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1614,"ST",1,"LVM",100,1,"1LE15031DA222GB7"]
["1LE1503-1DA22-2JB4","SIMOTICS SD MOTOR TYPE: 1CV3162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1567,"ST",1,"LVM",100,1,"1LE15031DA222JB4"]
["1LE1503-1CA13-4GB5","SIMOTICS SD MOTOR TYPE: 1CV3131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",1212,"ST",1,"LVM",73,1,"1LE15031CA134GB5"]
["1LE1503-1DA32-2JA6","SIMOTICS SD MOTOR TYPE: 1CV3163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box on left-hand side",1983,"ST",1,"LVM",110,1,"1LE15031DA322JA6"]
["1LE1503-1DA40-4GB4","SIMOTICS SD MOTOR TYPE: 1CV3164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2344,"ST",1,"LVM",127,1,"1LE15031DA404GB4"]
["1LE1503-1DA43-3GB6","SIMOTICS SD MOTOR TYPE: 1CV3164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",2443,"ST",1,"LVM",127,1,"1LE15031DA433GB6"]
["1LE1503-1EA20-4GB6","SIMOTICS SD MOTOR TYPE: 1CV3182A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 180M, * 22kW (50 Hz) 24.5kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",2751,"ST",1,"LVM",160,1,"1LE15031EA204GB6"]
["1LE1503-1EA23-3GA5","SIMOTICS SD MOTOR TYPE: 1CV3182A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 180M, * 22kW (50 Hz) 24.5kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF300 (A350) without motor protection Terminal box on RHS",2734,"ST",1,"LVM",160,1,"1LE15031EA233GA5"]
["1LE1503-1EB22-2AA5","SIMOTICS SD MOTOR TYPE: 1CV3182B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 4-pole * Size 180M, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 without motor protection Terminal box on RHS",2202,"ST",1,"LVM",165,1,"1LE15031EB222AA5"]
["1LE1503-1EB23-3GB5","SIMOTICS SD MOTOR TYPE: 1CV3182B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 4-pole * Size 180M, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",2448,"ST",1,"LVM",165,1,"1LE15031EB233GB5"]
["1LE1503-1EB23-4GC4","SIMOTICS SD MOTOR TYPE: 1CV3182B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 4-pole * Size 180M, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",2335,"ST",1,"LVM",165,1,"1LE15031EB234GC4"]
["1LE1503-1EB43-4FC6","SIMOTICS SD MOTOR TYPE: 1CV3184B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 4-pole * Size 180L, * 22kW (50 Hz) 25.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",2823,"ST",1,"LVM",170,1,"1LE15031EB434FC6"]
["1LE1503-1EB43-4WB4","SIMOTICS SD MOTOR TYPE: 1CV3184B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 4-pole * Size 180L, * 22kW (50 Hz) 25.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF300 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2606,"ST",1,"LVM",170,1,"1LE15031EB434WB4"]
["1LE1503-1EC43-3AB5","SIMOTICS SD MOTOR TYPE: 1CV3184C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 180L, * 15kW (50 Hz) 18kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",2852,"ST",1,"LVM",180,1,"1LE15031EC433AB5"]
["1LE1503-1EC43-4FC4","SIMOTICS SD MOTOR TYPE: 1CV3184C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 180L, * 15kW (50 Hz) 18kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",2827,"ST",1,"LVM",180,1,"1LE15031EC434FC4"]
["1LE1503-2AA43-3FB4","SIMOTICS SD MOTOR TYPE: 1CV3204A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 200L, * 30kW (50 Hz) 33.5kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 5, flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",3429,"ST",1,"LVM",225,1,"1LE15032AA433FB4"]
["1LE1503-2AA43-4WC5","SIMOTICS SD MOTOR TYPE: 1CV3204A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 200L, * 30kW (50 Hz) 33.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF350 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",3686,"ST",1,"LVM",225,1,"1LE15032AA434WC5"]
["1LE1503-2AA53-3GB6","SIMOTICS SD MOTOR TYPE: 1CV3205A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 200L, * 37kW (50 Hz) 41.5kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",4410,"ST",1,"LVM",250,1,"1LE15032AA533GB6"]
["1LE1503-2AA53-4GC6","SIMOTICS SD MOTOR TYPE: 1CV3205A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 200L, * 37kW (50 Hz) 41.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF350 (A400) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",4420,"ST",1,"LVM",250,1,"1LE15032AA534GC6"]
["1LE1503-2AB52-2WB4","SIMOTICS SD MOTOR TYPE: 1CV3205B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 200L, * 30kW (50 Hz) 34.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 15 * Flange: FF350 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",3384,"ST",1,"LVM",240,1,"1LE15032AB522WB4"]
["1LE1503-2AB53-4JC4","SIMOTICS SD MOTOR TYPE: 1CV3205B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 200L, * 30kW (50 Hz) 34.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF350 (A400) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",3437,"ST",1,"LVM",240,1,"1LE15032AB534JC4"]
["1LE1503-2AC43-3GB4","SIMOTICS SD MOTOR TYPE: 1CV3204C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 200L, * 18.5 kW (50 Hz) 22 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",3403,"ST",1,"LVM",215,1,"1LE15032AC433GB4"]
["1LE1503-2AC50-4JA6","SIMOTICS SD MOTOR TYPE: 1CV3205C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 200L, * 22kW (50 Hz) 26.5kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF350 (A400) without motor protection Terminal box on left-hand side",3947,"ST",1,"LVM",230,1,"1LE15032AC504JA6"]
["1LE1503-2AC53-3FB5","SIMOTICS SD MOTOR TYPE: 1CV3205C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 200L, * 22kW (50 Hz) 26.5kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 5, flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",4075,"ST",1,"LVM",230,1,"1LE15032AC533FB5"]
["1LE1503-2AC53-4JC5","SIMOTICS SD MOTOR TYPE: 1CV3205C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 200L, * 22kW (50 Hz) 26.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF350 (A400) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",4124,"ST",1,"LVM",230,1,"1LE15032AC534JC5"]
["1LE1503-2BA22-1AB5","SIMOTICS SD MOTOR TYPE: 1CV3222A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 225M * 45kW (50 Hz) 51kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",4854,"ST",1,"LVM",315,1,"1LE15032BA221AB5"]
["1LE1503-2BA23-4JA4","SIMOTICS SD MOTOR TYPE: 1CV3222A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 225M * 45kW (50 Hz) 51kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF400 (A450) without motor protection Terminal box at top",4631,"ST",1,"LVM",315,1,"1LE15032BA234JA4"]
["1LE1503-2BB02-1WB4","SIMOTICS SD MOTOR TYPE: 1CV3220B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 225S * 37kW (50 Hz) 42.5kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 15 * Flange: FF400 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",4052,"ST",1,"LVM",285,1,"1LE15032BB021WB4"]
["1LE1503-2BB03-4WC5","SIMOTICS SD MOTOR TYPE: 1CV3220B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 225S * 37kW (50 Hz) 42.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF400 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",4272,"ST",1,"LVM",285,1,"1LE15032BB034WC5"]
["1LE1503-2BB22-1FA6","SIMOTICS SD MOTOR TYPE: 1CV3222B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 225M * 45kW (50 Hz) 52kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF400 (A450) without motor protection Terminal box on left-hand side",4639,"ST",1,"LVM",320,1,"1LE15032BB221FA6"]
["1LE1503-2BB23-4JA5","SIMOTICS SD MOTOR TYPE: 1CV3222B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 225M * 45kW (50 Hz) 52kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF400 (A450) without motor protection Terminal box on RHS",4592,"ST",1,"LVM",320,1,"1LE15032BB234JA5"]
["1LE1503-2BC20-4JA5","SIMOTICS SD MOTOR TYPE: 1CV3222C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 225M * 30kW (50 Hz) 36 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF400 (A450) without motor protection Terminal box on RHS",4974,"ST",1,"LVM",325,1,"1LE15032BC204JA5"]
["1LE1503-2BC23-4GC5","SIMOTICS SD MOTOR TYPE: 1CV3222C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 225M * 30kW (50 Hz) 36 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF400 (A450) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",5162,"ST",1,"LVM",325,1,"1LE15032BC234GC5"]
["1LE1503-2CA22-1AA6","SIMOTICS SD MOTOR TYPE: 1CV3252A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 250M * 55kW (50 Hz) 62kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, without motor protection Terminal box on left-hand side",5718,"ST",1,"LVM",385,1,"1LE15032CA221AA6"]
["1LE1503-2CA23-4FB5","SIMOTICS SD MOTOR TYPE: 1CV3252A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 250M * 55kW (50 Hz) 62kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",5964,"ST",1,"LVM",385,1,"1LE15032CA234FB5"]
["1LE1503-2CB20-4AB6","SIMOTICS SD MOTOR TYPE: 1CV3252B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 250M * 55kW (50 Hz) 63kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",5458,"ST",1,"LVM",420,1,"1LE15032CB204AB6"]
["1LE1503-2CB23-4GB5","SIMOTICS SD MOTOR TYPE: 1CV3252B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 250M * 55kW (50 Hz) 63kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",5675,"ST",1,"LVM",420,1,"1LE15032CB234GB5"]
["1LE1503-2CC20-4FA4","SIMOTICS SD MOTOR TYPE: 1CV3252C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 250M * 37kW (50 Hz) 44.5kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF500 (A550) without motor protection Terminal box at top",5799,"ST",1,"LVM",405,1,"1LE15032CC204FA4"]
["1LE1503-2CC23-4JB6","SIMOTICS SD MOTOR TYPE: 1CV3252C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 250M * 37kW (50 Hz) 44.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",6354,"ST",1,"LVM",405,1,"1LE15032CC234JB6"]
["1LE1503-2DA02-1AA4","SIMOTICS SD MOTOR TYPE: 1CV3280A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 280S, * 75kW (50 Hz) 84kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, without motor protection Terminal box at top",7232,"ST",1,"LVM",510,1,"1LE15032DA021AA4"]
["1LE1503-2CB23-4JA4","SIMOTICS SD MOTOR TYPE: 1CV3252B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 250M * 55kW (50 Hz) 63kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF500 (A550) without motor protection Terminal box at top",5307,"ST",1,"LVM",420,1,"1LE15032CB234JA4"]
["1LE1503-2DA20-4GA5","SIMOTICS SD MOTOR TYPE: 1CV3282A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 280M * 90kW (50 Hz) 101kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF500 (A550) without motor protection Terminal box on RHS",9075,"ST",1,"LVM",590,1,"1LE15032DA204GA5"]
["1LE1503-2DA23-4GA4","SIMOTICS SD MOTOR TYPE: 1CV3282A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 280M * 90kW (50 Hz) 101kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF500 (A550) without motor protection Terminal box at top",8712,"ST",1,"LVM",590,1,"1LE15032DA234GA4"]
["1LE1503-2DB00-4JA4","SIMOTICS SD MOTOR TYPE: 1CV3280B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 280S, * 75kW (50 Hz) 86kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF500 (A550) without motor protection Terminal box at top",7118,"ST",1,"LVM",570,1,"1LE15032DB004JA4"]
["1LE1503-2DB02-2GC6","SIMOTICS SD MOTOR TYPE: 1CV3280B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 280S, * 75kW (50 Hz) 86kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF500 (A550) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",7680,"ST",1,"LVM",570,1,"1LE15032DB022GC6"]
["1LE1503-2DB22-1FB6","SIMOTICS SD MOTOR TYPE: 1CV3282B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 280M * 90kW (50 Hz) 104kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",8873,"ST",1,"LVM",670,1,"1LE15032DB221FB6"]
["1LE1503-2DB23-3JA5","SIMOTICS SD MOTOR TYPE: 1CV3282B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 280M * 90kW (50 Hz) 104kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF500 (A550) without motor protection Terminal box on RHS",8789,"ST",1,"LVM",670,1,"1LE15032DB233JA5"]
["1LE1503-2DC02-2AB5","SIMOTICS SD MOTOR TYPE: 1CV3280C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 280S, * 45kW (50 Hz) 54kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",7253,"ST",1,"LVM",510,1,"1LE15032DC022AB5"]
["1LE1503-2DC03-3FA6","SIMOTICS SD MOTOR TYPE: 1CV3280C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 280S, * 45kW (50 Hz) 54kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 5, flange: FF500 (A550) without motor protection Terminal box on left-hand side",7526,"ST",1,"LVM",510,1,"1LE15032DC033FA6"]
["1LE1503-2DC22-2AC6","SIMOTICS SD MOTOR TYPE: 1CV3282C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 280M * 55kW (50 Hz) 66kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",8544,"ST",1,"LVM",560,1,"1LE15032DC222AC6"]
["1LE1503-2DC23-3AB5","SIMOTICS SD MOTOR TYPE: 1CV3282C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 280M * 55kW (50 Hz) 66kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",8563,"ST",1,"LVM",560,1,"1LE15032DC233AB5"]
["1LE1503-3AA02-2GC5","SIMOTICS SD MOTOR TYPE: 1CV3310A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 315S, * 110kW (50 Hz) 123kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, Flange: FF600 (A660) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",11228,"ST",1,"LVM",750,1,"1LE15033AA022GC5"]
["1LE1503-3AA03-3JB5","SIMOTICS SD MOTOR TYPE: 1CV3310A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 315S, * 110kW (50 Hz) 123kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",11345,"ST",1,"LVM",750,1,"1LE15033AA033JB5"]
["1LE1503-3AA22-2AB6","SIMOTICS SD MOTOR TYPE: 1CV3312A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 315M, * 132kW (50 Hz) 148kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",12684,"ST",1,"LVM",880,1,"1LE15033AA222AB6"]
["1LE1503-3AA23-4JA5","SIMOTICS SD MOTOR TYPE: 1CV3312A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 315M, * 132kW (50 Hz) 148kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF600 (A660) without motor protection Terminal box on RHS",13018,"ST",1,"LVM",880,1,"1LE15033AA234JA5"]
["1LE1503-3AA43-4JC5","SIMOTICS SD MOTOR TYPE: 1CV3314A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 315L, * 160kW (50 Hz) 180kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF600 (A660) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",16201,"ST",1,"LVM",980,1,"1LE15033AA434JC5"]
["1LE1503-3AA52-1JB4","SIMOTICS SD MOTOR TYPE: 1CV3315A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 315L, * 200kW (50 Hz) 224kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",19580,"ST",1,"LVM",1150,1,"1LE15033AA521JB4"]
["1LE1503-3AB02-2FB6","SIMOTICS SD MOTOR TYPE: 1CV3310B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 4-pole * Size 315S, * 110kW (50 Hz) 127kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",10899,"ST",1,"LVM",760,1,"1LE15033AB022FB6"]
["1LE1503-3AB02-2GB6","SIMOTICS SD MOTOR TYPE: 1CV3310B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 4-pole * Size 315S, * 110kW (50 Hz) 127kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",10903,"ST",1,"LVM",760,1,"1LE15033AB022GB6"]
["1LE1503-3AB20-4AA4","SIMOTICS SD MOTOR TYPE: 1CV3312B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 4-pole * Size 315M, * 132kW (50 Hz) 152kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box at top",11634,"ST",1,"LVM",960,1,"1LE15033AB204AA4"]
["1LE1503-3AB23-4AB6","SIMOTICS SD MOTOR TYPE: 1CV3312B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 4-pole * Size 315M, * 132kW (50 Hz) 152kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",12222,"ST",1,"LVM",960,1,"1LE15033AB234AB6"]
["1LE1503-3AB43-3JB6","SIMOTICS SD MOTOR TYPE: 1CV3314B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 4-pole * Size 315L, * 160kW (50 Hz) 184kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",15377,"ST",1,"LVM",990,1,"1LE15033AB433JB6"]
["1LE1503-3AB52-1JB5","SIMOTICS SD MOTOR TYPE: 1CV3315B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 315L, * 200kW (50 Hz) 230kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",18779,"ST",1,"LVM",1190,1,"1LE15033AB521JB5"]
["1LE1503-3AB53-3GA4","SIMOTICS SD MOTOR TYPE: 1CV3315B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 315L, * 200kW (50 Hz) 230kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, Flange: FF600 (A660) without motor protection Terminal box at top",18133,"ST",1,"LVM",1190,1,"1LE15033AB533GA4"]
["1LE1503-3AC02-1JB4","SIMOTICS SD MOTOR TYPE: 1CV3310C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 6-pole * Size 315S, * 75kW (50 Hz) 90 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",11558,"ST",1,"LVM",750,1,"1LE15033AC021JB4"]
["1LE1503-3AC22-2AB4","SIMOTICS SD MOTOR TYPE: 1CV3312C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 315M, * 90kW (50 Hz) 108kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",12267,"ST",1,"LVM",890,1,"1LE15033AC222AB4"]
["1LE1503-3AC53-3AB5","SIMOTICS SD MOTOR TYPE: 1CV3315C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 315L, * 132kW (50 Hz) 158kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",18065,"ST",1,"LVM",1110,1,"1LE15033AC533AB5"]
["1LE1503-3AC62-2GC5","SIMOTICS SD MOTOR TYPE: 1CV3316C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 315L, * 160kW (50 Hz) 192kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, Flange: FF600 (A660) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",22148,"ST",1,"LVM",1160,1,"1LE15033AC622GC5"]
["1LE1504-1CA13-4JC4","SIMOTICS SD MOTOR TYPE: 1CV4131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",1412,"ST",1,"LVM",74,1,"1LE15041CA134JC4"]
["1LE1504-1DA42-1GA6","SIMOTICS SD MOTOR TYPE: 1CV4164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF300 (A350) without motor protection Terminal box on left-hand side",2829,"ST",1,"LVM",147,1,"1LE15041DA421GA6"]
["1LE1504-1EA22-2GA5","SIMOTICS SD MOTOR TYPE: 1CV4182A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 180M, * 22kW (50 Hz) 24.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF300 (A350) without motor protection Terminal box on RHS",3192,"ST",1,"LVM",175,1,"1LE15041EA222GA5"]
["1LE1504-1EA23-3FB6","SIMOTICS SD MOTOR TYPE: 1CV4182A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 180M, * 22kW (50 Hz) 24.5kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",3351,"ST",1,"LVM",175,1,"1LE15041EA233FB6"]
["1LE1504-1EA23-4GC6","SIMOTICS SD MOTOR TYPE: 1CV4182A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 180M, * 22kW (50 Hz) 24.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",3369,"ST",1,"LVM",175,1,"1LE15041EA234GC6"]
["1LE1504-1EB22-2WC6","SIMOTICS SD MOTOR TYPE: 1CV4182B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 180M, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 15 * Flange: FF300 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",2964,"ST",1,"LVM",187,1,"1LE15041EB222WC6"]
["1LE1504-1EB40-4GB4","SIMOTICS SD MOTOR TYPE: 1CV4184B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 180L, * 22kW (50 Hz) 25.3kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",3069,"ST",1,"LVM",192,1,"1LE15041EB404GB4"]
["1LE1504-1EB43-3FA4","SIMOTICS SD MOTOR TYPE: 1CV4184B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 180L, * 22kW (50 Hz) 25.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",3028,"ST",1,"LVM",192,1,"1LE15041EB433FA4"]
["1LE1504-1EB43-4FB4","SIMOTICS SD MOTOR TYPE: 1CV4184B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 180L, * 22kW (50 Hz) 25.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",3070,"ST",1,"LVM",192,1,"1LE15041EB434FB4"]
["1LE1504-2AA42-2JB4","SIMOTICS SD MOTOR TYPE: 1CV4204A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 200L, * 30kW (50 Hz) 33.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",3998,"ST",1,"LVM",222,1,"1LE15042AA422JB4"]
["1LE1504-2AA43-4GA4","SIMOTICS SD MOTOR TYPE: 1CV4204A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 200L, * 30kW (50 Hz) 33.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF350 (A400) without motor protection Terminal box at top",3858,"ST",1,"LVM",222,1,"1LE15042AA434GA4"]
["1LE1504-2AA53-3GA6","SIMOTICS SD MOTOR TYPE: 1CV4205A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 200L, * 37kW (50 Hz) 41.5kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF350 (A400) without motor protection Terminal box on left-hand side",5049,"ST",1,"LVM",263,1,"1LE15042AA533GA6"]
["1LE1504-2AA53-4FA6","SIMOTICS SD MOTOR TYPE: 1CV4205A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 200L, * 37kW (50 Hz) 41.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF350 (A400) without motor protection Terminal box on left-hand side",4983,"ST",1,"LVM",263,1,"1LE15042AA534FA6"]
["1LE1504-2AB52-2GC6","SIMOTICS SD MOTOR TYPE: 1CV4205B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 200L, * 30kW (50 Hz) 34.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF350 (A400) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",4176,"ST",1,"LVM",258,1,"1LE15042AB522GC6"]
["1LE1504-2AB53-3JA4","SIMOTICS SD MOTOR TYPE: 1CV4205B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 200L, * 30kW (50 Hz) 34.5kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF350 (A400) without motor protection Terminal box at top",3923,"ST",1,"LVM",258,1,"1LE15042AB533JA4"]
["1LE1504-2BA22-2GC6","SIMOTICS SD MOTOR TYPE: 1CV4222A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 225M * 45kW (50 Hz) 51kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF400 (A450) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",5708,"ST",1,"LVM",330,1,"1LE15042BA222GC6"]
["1LE1504-2BA23-3GA5","SIMOTICS SD MOTOR TYPE: 1CV4222A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 225M * 45kW (50 Hz) 51kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF400 (A450) without motor protection Terminal box on RHS",5568,"ST",1,"LVM",330,1,"1LE15042BA233GA5"]
["1LE1504-2BB00-4GA6","SIMOTICS SD MOTOR TYPE: 1CV4220B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 225S * 37kW (50 Hz) 42.5kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF400 (A450) without motor protection Terminal box on left-hand side",4503,"ST",1,"LVM",345,1,"1LE15042BB004GA6"]
["1LE1504-2BB03-3JA4","SIMOTICS SD MOTOR TYPE: 1CV4220B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 225S * 37kW (50 Hz) 42.5kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF400 (A450) without motor protection Terminal box at top",4419,"ST",1,"LVM",345,1,"1LE15042BB033JA4"]
["1LE1504-2BB22-2FA5","SIMOTICS SD MOTOR TYPE: 1CV4222B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 60 Hz, P60: IE3 4-pole * Size 225M * 45kW (50 Hz) 52kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF400 (A450) without motor protection Terminal box on RHS",5183,"ST",1,"LVM",415,1,"1LE15042BB222FA5"]
["1LE1504-2BB23-3JB6","SIMOTICS SD MOTOR TYPE: 1CV4222B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 60 Hz, P60: IE3 4-pole * Size 225M * 45kW (50 Hz) 52kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF400 (A450) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",5453,"ST",1,"LVM",415,1,"1LE15042BB233JB6"]
["1LE1504-2CA22-2AC5","SIMOTICS SD MOTOR TYPE: 1CV4252A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 250M * 55kW (50 Hz) 62kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",6601,"ST",1,"LVM",430,1,"1LE15042CA222AC5"]
["1LE1504-2CA23-4FC6","SIMOTICS SD MOTOR TYPE: 1CV4252A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 250M * 55kW (50 Hz) 62kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF500 (A550) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",6814,"ST",1,"LVM",430,1,"1LE15042CA234FC6"]
["1LE1504-2CA23-4JA4","SIMOTICS SD MOTOR TYPE: 1CV4252A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 250M * 55kW (50 Hz) 62kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF500 (A550) without motor protection Terminal box at top",6357,"ST",1,"LVM",430,1,"1LE15042CA234JA4"]
["1LE1504-2CB23-3AA5","SIMOTICS SD MOTOR TYPE: 1CV4252B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 250M * 55kW (50 Hz) 63kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, without motor protection Terminal box on RHS",6222,"ST",1,"LVM",490,1,"1LE15042CB233AA5"]
["1LE1504-2CB23-4JB5","SIMOTICS SD MOTOR TYPE: 1CV4252B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 250M * 55kW (50 Hz) 63kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",6564,"ST",1,"LVM",490,1,"1LE15042CB234JB5"]
["1LE1504-2DA03-3FA4","SIMOTICS SD MOTOR TYPE: 1CV4280A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 280S, * 75kW (50 Hz) 84kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 5, flange: FF500 (A550) without motor protection Terminal box at top",8676,"ST",1,"LVM",600,1,"1LE15042DA033FA4"]
["1LE1504-2DA03-4WC5","SIMOTICS SD MOTOR TYPE: 1CV4280A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 280S, * 75kW (50 Hz) 84kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF500 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",9405,"ST",1,"LVM",600,1,"1LE15042DA034WC5"]
["1LE1504-2DA23-3GB4","SIMOTICS SD MOTOR TYPE: 1CV4282A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 280M * 90kW (50 Hz) 101kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",10276,"ST",1,"LVM",610,1,"1LE15042DA233GB4"]
["1LE1504-2DA23-4GC5","SIMOTICS SD MOTOR TYPE: 1CV4282A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 280M * 90kW (50 Hz) 101kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF500 (A550) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",10620,"ST",1,"LVM",610,1,"1LE15042DA234GC5"]
["1LE1504-2DB03-4FB5","SIMOTICS SD MOTOR TYPE: 1CV4280B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 280S, * 75kW (50 Hz) 86kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",8613,"ST",1,"LVM",670,1,"1LE15042DB034FB5"]
["1LE1504-2DB20-4AB5","SIMOTICS SD MOTOR TYPE: 1CV4282B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 280M * 90kW (50 Hz) 104kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",9521,"ST",1,"LVM",730,1,"1LE15042DB204AB5"]
["1LE1504-2DB23-4GA6","SIMOTICS SD MOTOR TYPE: 1CV4282B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 280M * 90kW (50 Hz) 104kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF500 (A550) without motor protection Terminal box on left-hand side",9663,"ST",1,"LVM",730,1,"1LE15042DB234GA6"]
["1LE1504-3AA02-1AB6","SIMOTICS SD MOTOR TYPE: 1CV4310A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 315S, * 110kW (50 Hz) 123kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",12185,"ST",1,"LVM",750,1,"1LE15043AA021AB6"]
["1LE1504-3AA03-4JB4","SIMOTICS SD MOTOR TYPE: 1CV4310A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 315S, * 110kW (50 Hz) 123kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",12099,"ST",1,"LVM",750,1,"1LE15043AA034JB4"]
["1LE1504-3AA22-1FB4","SIMOTICS SD MOTOR TYPE: 1CV4312A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 315M, * 132kW (50 Hz) 148kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",14435,"ST",1,"LVM",980,1,"1LE15043AA221FB4"]
["1LE1504-3AA42-1JB4","SIMOTICS SD MOTOR TYPE: 1CV4314A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 315L, * 160kW (50 Hz) 180kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",17900,"ST",1,"LVM",1060,1,"1LE15043AA421JB4"]
["1LE1504-3AA43-3AB4","SIMOTICS SD MOTOR TYPE: 1CV4314A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 315L, * 160kW (50 Hz) 180kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",17396,"ST",1,"LVM",1060,1,"1LE15043AA433AB4"]
["1LE1504-3AA53-3JB4","SIMOTICS SD MOTOR TYPE: 1CV4315A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 315L, * 200kW (50 Hz) 224kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",22100,"ST",1,"LVM",1180,1,"1LE15043AA533JB4"]
["1LE1504-3AB00-4GB4","SIMOTICS SD MOTOR TYPE: 1CV4310B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 315M, * 110kW (50 Hz) 127kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",11788,"ST",1,"LVM",910,1,"1LE15043AB004GB4"]
["1LE1504-3AB03-4GB5","SIMOTICS SD MOTOR TYPE: 1CV4310B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 315M, * 110kW (50 Hz) 127kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",12205,"ST",1,"LVM",910,1,"1LE15043AB034GB5"]
["1LE1504-3AB22-1GB6","SIMOTICS SD MOTOR TYPE: 1CV4312B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 315M, * 132kW (50 Hz) 152kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",14310,"ST",1,"LVM",990,1,"1LE15043AB221GB6"]
["1LE1504-3AB22-2AC6","SIMOTICS SD MOTOR TYPE: 1CV4312B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 315M, * 132kW (50 Hz) 152kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",13807,"ST",1,"LVM",990,1,"1LE15043AB222AC6"]
["1LE1504-3AB42-2JC5","SIMOTICS SD MOTOR TYPE: 1CV4314B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 315L, * 160kW (50 Hz) 184kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF600 (A660) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",17083,"ST",1,"LVM",1220,1,"1LE15043AB422JC5"]
["1LE1504-3AB43-4GB4","SIMOTICS SD MOTOR TYPE: 1CV4314B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 315L, * 160kW (50 Hz) 184kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",16492,"ST",1,"LVM",1220,1,"1LE15043AB434GB4"]
["1LE1504-3AB53-4GC5","SIMOTICS SD MOTOR TYPE: 1CV4315B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 315L, * 200kW (50 Hz) 230kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, Flange: FF600 (A660) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",20888,"ST",1,"LVM",1380,1,"1LE15043AB534GC5"]
["1LE1523-1CB02-2VA5","SIMOTICS SD MOTOR TYPE: 1CV3130B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line IE3, NEMA Premium, CSA, UL, 4-pole * Size 132S, * 5.5kW (50 Hz) NEMA 60Hz: 7.5 HP 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 8, without motor protection Terminal box on RHS",1027,"ST",1,"LVM",74,1,"1LE15231CB022VA5"]
["1LE1601-1EA22-2JC4","SIMOTICS SD MOTOR TYPE: 1CV2182A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 180M, * 22kW (50 Hz) 24.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",2712,"ST",1,"LVM",145,1,"1LE16011EA222JC4"]
["1LE1601-1EB22-1AB6","SIMOTICS SD MOTOR TYPE: 1CV2182B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 180M, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",2252,"ST",1,"LVM",160,1,"1LE16011EB221AB6"]
["1LE1601-1EC42-1AB5","SIMOTICS SD MOTOR TYPE: 1CV2184C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 6-pole * Size 180L, * 15kW (50 Hz) 18kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",2739,"ST",1,"LVM",155,1,"1LE16011EC421AB5"]
["1LE1601-1EC43-3GB6","SIMOTICS SD MOTOR TYPE: 1CV2184C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 6-pole * Size 180L, * 15kW (50 Hz) 18kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",2851,"ST",1,"LVM",155,1,"1LE16011EC433GB6"]
["1LE1601-2AA53-4AC5","SIMOTICS SD MOTOR TYPE: 1CV2205A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 200L, * 37kW (50 Hz) 41.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",4271,"ST",1,"LVM",225,1,"1LE16012AA534AC5"]
["1LE1601-2AB52-2AB5","SIMOTICS SD MOTOR TYPE: 1CV2205B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 200L, * 30kW (50 Hz) 34.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",3254,"ST",1,"LVM",230,1,"1LE16012AB522AB5"]
["1LE1601-2AC50-4AB6","SIMOTICS SD MOTOR TYPE: 1CV2205C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 200L, * 22kW (50 Hz) 26.5kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",3758,"ST",1,"LVM",220,1,"1LE16012AC504AB6"]
["1LE1601-2AC53-3JB5","SIMOTICS SD MOTOR TYPE: 1CV2205C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 200L, * 22kW (50 Hz) 26.5kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",4001,"ST",1,"LVM",220,1,"1LE16012AC533JB5"]
["1LE1601-2BB03-4AC4","SIMOTICS SD MOTOR TYPE: 1CV2220B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 225S * 37kW (50 Hz) 42.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",3830,"ST",1,"LVM",280,1,"1LE16012BB034AC4"]
["1LE1601-2BB02-1JB4","SIMOTICS SD MOTOR TYPE: 1CV2220B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 225S * 37kW (50 Hz) 42.5kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF400 (A450) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",3911,"ST",1,"LVM",280,1,"1LE16012BB021JB4"]
["1LE1601-2BC20-4JB4","SIMOTICS SD MOTOR TYPE: 1CV2222C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 225M * 30kW (50 Hz) 36 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF400 (A450) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",4841,"ST",1,"LVM",300,1,"1LE16012BC204JB4"]
["1LE1601-2CA23-4GC4","SIMOTICS SD MOTOR TYPE: 1CV2252A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 250M * 55kW (50 Hz) 62kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF500 (A550) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",5866,"ST",1,"LVM",360,1,"1LE16012CA234GC4"]
["1LE1601-2CC22-2GC6","SIMOTICS SD MOTOR TYPE: 1CV2252C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 250M * 37kW (50 Hz) 44.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF500 (A550) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",6440,"ST",1,"LVM",370,1,"1LE16012CC222GC6"]
["1LE1601-2DA02-2JB5","SIMOTICS SD MOTOR TYPE: 1CV2280A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 280S, * 75kW (50 Hz) 84kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",7606,"ST",1,"LVM",490,1,"1LE16012DA022JB5"]
["1LE1601-2DA20-4GB6","SIMOTICS SD MOTOR TYPE: 1CV2282A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 280M * 90kW (50 Hz) 101kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",8949,"ST",1,"LVM",530,1,"1LE16012DA204GB6"]
["1LE1601-2DB20-4JB5","SIMOTICS SD MOTOR TYPE: 1CV2282B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 280M * 90kW (50 Hz) 104kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",8404,"ST",1,"LVM",570,1,"1LE16012DB204JB5"]
["1LE1601-2DB23-3GB5","SIMOTICS SD MOTOR TYPE: 1CV2282B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 280M * 90kW (50 Hz) 104kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",8452,"ST",1,"LVM",570,1,"1LE16012DB233GB5"]
["1LE1601-2DC03-4JC5","SIMOTICS SD MOTOR TYPE: 1CV2280C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 280S, * 45kW (50 Hz) 54kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF500 (A550) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",7471,"ST",1,"LVM",460,1,"1LE16012DC034JC5"]
["1LE1601-3AA02-2AB4","SIMOTICS SD MOTOR TYPE: 1CV2310A low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 315S, * 110kW (50 Hz) 123kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",9996,"ST",1,"LVM",720,1,"1LE16013AA022AB4"]
["1LE1601-3AA40-4GB6","SIMOTICS SD MOTOR TYPE: 1CV2314A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 315L, * 160kW (50 Hz) 180kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",15832,"ST",1,"LVM",930,1,"1LE16013AA404GB6"]
["1LE1601-3AA43-4JB5","SIMOTICS SD MOTOR TYPE: 1CV2314A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 315L, * 160kW (50 Hz) 180kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",15706,"ST",1,"LVM",930,1,"1LE16013AA434JB5"]
["1LE1601-3AB22-2JB5","SIMOTICS SD MOTOR TYPE: 1CV2312B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 315M, * 132kW (50 Hz) 152kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",12178,"ST",1,"LVM",870,1,"1LE16013AB222JB5"]
["1LE1601-3AB23-4AC4","SIMOTICS SD MOTOR TYPE: 1CV2312B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 315M, * 132kW (50 Hz) 152kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",11542,"ST",1,"LVM",870,1,"1LE16013AB234AC4"]
["1LE1601-3AB43-4GC6","SIMOTICS SD MOTOR TYPE: 1CV2314B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 315L, * 160kW (50 Hz) 184kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, Flange: FF600 (A660) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",14714,"ST",1,"LVM",940,1,"1LE16013AB434GC6"]
["1LE1601-3AC03-3JB4","SIMOTICS SD MOTOR TYPE: 1CV2310C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 315S, * 75kW (50 Hz) 90 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",11010,"ST",1,"LVM",660,1,"1LE16013AC033JB4"]
["1LE1601-3AC22-2JB5","SIMOTICS SD MOTOR TYPE: 1CV2312C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 315M, * 90kW (50 Hz) 108kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",12556,"ST",1,"LVM",730,1,"1LE16013AC222JB5"]
["1LE1601-3AC52-2AB6","SIMOTICS SD MOTOR TYPE: 1CV2315C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations to be considered! 6-pole * Size 315L, * 132kW (50 Hz) 158kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",17176,"ST",1,"LVM",990,1,"1LE16013AC522AB6"]
["1LE1603-1AA43-4GB6","SIMOTICS SD MOTOR TYPE: 1CV3104A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",683,"ST",1,"LVM",36,1,"1LE16031AA434GB6"]
["1LE1603-1BA20-4GB5","SIMOTICS SD MOTOR TYPE: 1CV3112A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",813,"ST",1,"LVM",45,1,"1LE16031BA204GB5"]
["1LE1603-1BA23-4GC7","SIMOTICS SD MOTOR TYPE: 1CV3112A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF215 (A250) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",899,"ST",1,"LVM",45,1,"1LE16031BA234GC7"]
["1LE1603-1CA12-1GB6","SIMOTICS SD MOTOR TYPE: 1CV3131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1298,"ST",1,"LVM",73,1,"1LE16031CA121GB6"]
["1LE1603-1CA13-4GC7","SIMOTICS SD MOTOR TYPE: 1CV3131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",1378,"ST",1,"LVM",73,1,"1LE16031CA134GC7"]
["1LE1603-1DA32-1GB6","SIMOTICS SD MOTOR TYPE: 1CV3163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",2250,"ST",1,"LVM",110,1,"1LE16031DA321GB6"]
["1LE1603-1DA40-4GB6","SIMOTICS SD MOTOR TYPE: 1CV3164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",2614,"ST",1,"LVM",127,1,"1LE16031DA404GB6"]
["1LE1603-1EB22-1AB4","SIMOTICS SD MOTOR TYPE: 1CV3182B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 4-pole * Size 180M, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2272,"ST",1,"LVM",165,1,"1LE16031EB221AB4"]
["1LE1603-1EB23-3JB5","SIMOTICS SD MOTOR TYPE: 1CV3182B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 4-pole * Size 180M, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",2560,"ST",1,"LVM",165,1,"1LE16031EB233JB5"]
["1LE1603-1EC43-4GC4","SIMOTICS SD MOTOR TYPE: 1CV3184C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 180L, * 15kW (50 Hz) 18kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",3045,"ST",1,"LVM",180,1,"1LE16031EC434GC4"]
["1LE1603-2AB52-2GC4","SIMOTICS SD MOTOR TYPE: 1CV3205B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 200L, * 30kW (50 Hz) 34.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF350 (A400) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",3665,"ST",1,"LVM",240,1,"1LE16032AB522GC4"]
["1LE1603-2AC42-2JB5","SIMOTICS SD MOTOR TYPE: 1CV3204C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 200L, * 18.5 kW (50 Hz) 22 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",3733,"ST",1,"LVM",215,1,"1LE16032AC422JB5"]
["1LE1603-2AC53-4JC4","SIMOTICS SD MOTOR TYPE: 1CV3205C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 200L, * 22kW (50 Hz) 26.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF350 (A400) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",4260,"ST",1,"LVM",230,1,"1LE16032AC534JC4"]
["1LE1603-2BB23-4GC5","SIMOTICS SD MOTOR TYPE: 1CV3222B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 225M * 45kW (50 Hz) 52kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF400 (A450) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",5162,"ST",1,"LVM",320,1,"1LE16032BB234GC5"]
["1LE1603-2BC22-2JC6","SIMOTICS SD MOTOR TYPE: 1CV3222C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 225M * 30kW (50 Hz) 36 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF400 (A450) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",5582,"ST",1,"LVM",325,1,"1LE16032BC222JC6"]
["1LE1603-2CB20-4GB5","SIMOTICS SD MOTOR TYPE: 1CV3252B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 250M * 55kW (50 Hz) 63kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",6126,"ST",1,"LVM",420,1,"1LE16032CB204GB5"]
["1LE1603-2DB03-3AB5","SIMOTICS SD MOTOR TYPE: 1CV3280B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 280S, * 75kW (50 Hz) 86kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",7384,"ST",1,"LVM",570,1,"1LE16032DB033AB5"]
["1LE1603-2CC22-2AC6","SIMOTICS SD MOTOR TYPE: 1CV3252C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 250M * 37kW (50 Hz) 44.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",6559,"ST",1,"LVM",405,1,"1LE16032CC222AC6"]
["1LE1603-2DC02-2JC5","SIMOTICS SD MOTOR TYPE: 1CV3280C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 280S, * 45kW (50 Hz) 54kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF500 (A550) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",7891,"ST",1,"LVM",510,1,"1LE16032DC022JC5"]
["1LE1603-2DC22-2AB6","SIMOTICS SD MOTOR TYPE: 1CV3282C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 280M * 55kW (50 Hz) 66kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",8511,"ST",1,"LVM",560,1,"1LE16032DC222AB6"]
["1LE1603-3AB20-4GB4","SIMOTICS SD MOTOR TYPE: 1CV3312B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 4-pole * Size 315M, * 132kW (50 Hz) 152kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",12458,"ST",1,"LVM",960,1,"1LE16033AB204GB4"]
["1LE1603-3AB23-3GB4","SIMOTICS SD MOTOR TYPE: 1CV3312B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 4-pole * Size 315M, * 132kW (50 Hz) 152kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",12631,"ST",1,"LVM",960,1,"1LE16033AB233GB4"]
["1LE1603-3AB43-4GC5","SIMOTICS SD MOTOR TYPE: 1CV3314B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 4-pole * Size 315L, * 160kW (50 Hz) 184kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, Flange: FF600 (A660) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",15638,"ST",1,"LVM",990,1,"1LE16033AB434GC5"]
["1LE1603-3AC02-1JB4","SIMOTICS SD MOTOR TYPE: 1CV3310C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 6-pole * Size 315S, * 75kW (50 Hz) 90 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",11724,"ST",1,"LVM",750,1,"1LE16033AC021JB4"]
["1LE1603-3AC40-4AB4","SIMOTICS SD MOTOR TYPE: 1CV3314C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 315L, * 110kW (50 Hz) 132 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",14952,"ST",1,"LVM",990,1,"1LE16033AC404AB4"]
["1LE1603-3AC43-4GC5","SIMOTICS SD MOTOR TYPE: 1CV3314C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 315L, * 110kW (50 Hz) 132 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, Flange: FF600 (A660) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",16100,"ST",1,"LVM",990,1,"1LE16033AC434GC5"]
["1LE2121-1CA31-4AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR GENERAL PURPOSE GP100A ALUMINIUM HOUSING NP EFFICIENCY TEFC (IP55) 2 POLE * FS 184T 5 HP (60 HZ) 230/460V, 60HZ (suitable for 208V) FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",801,"ST",1,"LVM",30.4,1,"1LE21211CA314AA3"]
["1LE2121-2BC11-4EA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR GENERAL PURPOSE GP100A ALUMINIUM HOUSING NP EFFICIENCY TEFC (IP55) 6 POLE * FS 254T 7.5 HP (60 HZ) 230/460V, 60HZ (suitable for 208V) C-FACE WITH FEET WITHOUT WINDING PROTECTION FLOOR F-1",1911,"ST",1,"LVM",90.7,1,"1LE21212BC114EA3"]
["1LE2221-1CC11-3AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR GENERAL PURPOSE GP100 CAST-IRON HOUSING NP EFFICIENCY TEFC (IP55) 6 POLE * FS 182T 1.5 HP (60 HZ) 575V STD, 60HZ FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",651,"ST",1,"LVM",42.2,1,"1LE22211CC113AA3"]
["1LE2221-1CD31-4EA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR GENERAL PURPOSE GP100 CAST-IRON HOUSING NP EFFICIENCY TEFC (IP55) 8 POLE * FS 184T 1.5 HP (60 HZ) 230/460V, 60HZ (suitable for 208V) C-FACE WITH FEET WITHOUT WINDING PROTECTION FLOOR F-1",967,"ST",1,"LVM",44.9,1,"1LE22211CD314EA3"]
["1LE2221-2BA21-4EA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR GENERAL PURPOSE GP100 CAST-IRON HOUSING NP EFFICIENCY TEFC (IP55) 2 POLE * FS 256T 20 HP (60 HZ) 230/460V, 60HZ (suitable for 208V) C-FACE WITH FEET WITHOUT WINDING PROTECTION FLOOR F-1",2359,"ST",1,"LVM",132.9,1,"1LE22212BA214EA3"]
["1LE2221-4CC31-2AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR GENERAL PURPOSE GP100 CAST-IRON HOUSING BEARING DESIGN FOR INCREASED CANTILEVER FORCES NP EFFICIENCY TEFC (IP54) 6 POLE *  FS 447T 150 HP (60 HZ) 460V STD, 60HZ FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",19359,"ST",1,"LVM",889.05600000000004,1,"1LE22214CC312AA3"]
["1LE2311-2AA21-3GA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR SEVERE DUTY SD100 CAST-IRON HOUSING NPP EFFICIENCY TEFC (IP55) 2 POLE * FS 215T 10 HP (60 HZ) 575V STD, 60HZ C-FACE W/O FEET WITHOUT WINDING PROTECTION FLOOR F-1",1848,"ST",1,"LVM",88.9,1,"1LE23112AA213GA3"]
["1LE2321-1AA31-3GA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR SEVERE DUTY SD100 CAST-IRON HOUSING NP EFFICIENCY TEFC (IP55) 2 POLE * FS 145T 2 HP (60 HZ) 575V STD, 60HZ C-FACE W/O FEET WITHOUT WINDING PROTECTION FLOOR F-1",839,"ST",1,"LVM",32.700000000000003,1,"1LE23211AA313GA3"]
["1LE2321-1AB31-4GA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR SEVERE DUTY SD100 CAST-IRON HOUSING NP EFFICIENCY TEFC (IP55) 4 POLE * FS 145T 1.5 HP (60 HZ) 230/460V, 60HZ (SUITABLE FOR 208V) C-FACE W/O FEET WITHOUT WINDING PROTECTION FLOOR F-1",740,"ST",1,"LVM",36.299999999999997,1,"1LE23211AB314GA3"]
["1LE2321-3AD21-6AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR SEVERE DUTY SD100 CAST-IRON HOUSING NP EFFICIENCY TEFC (IP55) 8 POLE * FS 326T 25 HP (60 HZ) 230/460V, 60HZ FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",7006,"ST",1,"LVM",272.2,1,"1LE23213AD216AA3"]
["1LE2321-2AD21-3AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR SEVERE DUTY SD100 CAST-IRON HOUSING NP EFFICIENCY TEFC (IP55) 8 POLE * FS 215T 3 HP (60 HZ) 575V STD, 60HZ FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",1751,"ST",1,"LVM",71.7,1,"1LE23212AD213AA3"]
["1LE2321-4DD41-2AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR SEVERE DUTY SD100 CAST-IRON HOUSING NP EFFICIENCY TEFC (IP55) 8 POLE * FS 447TS 150 HP (60 HZ) 460V STD, 60HZ FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",30202,"ST",1,"LVM",1034.2,1,"1LE23214DD412AA3"]
["1LE2321-4ED21-3AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR SEVERE DUTY SD100 CAST-IRON HOUSING NP EFFICIENCY TEFC (IP55) 8 POLE * FS B445T 100 HP (60 HZ) 575V STD, 60HZ FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",22293,"ST",1,"LVM",861.8,1,"1LE23214ED213AA3"]
["1LE2421-1CA11-3AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR SEVERE DUTY SD100 IEEE 841, CAST-IRON HOUSING NP EFFICIENCY TEFC (IP55) 2 POLE * FS 182T 3 HP (60 HZ) 575V STD, 60HZ FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",1023,"ST",1,"LVM",48.5,1,"1LE24211CA113AA3"]
["1LE2421-2AD21-2AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR SEVERE DUTY SD100 IEEE 841, CAST-IRON HOUSING NP EFFICIENCY TEFC (IP55) 8 POLE * FS 215T 3 HP (60 HZ) 460V, 60HZ FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",2771,"ST",1,"LVM",72.599999999999994,1,"1LE24212AD212AA3"]
["1LE2421-4CB33-2AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR SEVERE DUTY SD100 IEEE 841, CAST-IRON HOUSING BEARING DESIGN FOR INCREASED CANTILEVER FORCES NP EFFICIENCY TEFC (IP55) 4 POLE *  FS 447T 200 HP (60 HZ) 460V,60Hz (Wye Start-Delta Run) FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",26105,"ST",1,"LVM",923.07600000000002,1,"1LE24214CB332AA3"]
["1LE2421-4DA21-3AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR SEVERE DUTY SD100 IEEE 841, CAST-IRON HOUSING NP EFFICIENCY TEFC (IP55) 2 POLE *  FS 445TS 150 HP (60 HZ) 575V STD, 60HZ FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",22718,"ST",1,"LVM",732.56399999999996,1,"1LE24214DA213AA3"]
["1LE5503-3AA63-3FB6","SIMOTICS SD MOTOR TYPE: 1CV3316A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F), according to 130(B) cast iron frame Basic Line Premium Efficiency IE3, 2-pole * Size 315L* 250 kW (50 Hz) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 5, Flange: FF740 (A800) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",23394,"ST",1,"LVM",1310,1,"1LE55033AA633FB6"]
["1LE5503-3AA63-4GC5","SIMOTICS SD MOTOR TYPE: 1CV3316A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F), according to 130(B) cast iron frame Basic Line Premium Efficiency IE3, 2-pole * Size 315L* 250 kW (50 Hz) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1, Flange: FF740 (A800) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",23339,"ST",1,"LVM",1310,1,"1LE55033AA634GC5"]
["1LE5503-3AA73-4GC6","SIMOTICS SD MOTOR TYPE: 1CV3317A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F), according to 130(B) cast iron frame Basic Line Premium Efficiency IE3, 2-pole * Size 315L* 315LkW (50 Hz) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1, Flange: FF740 (A800) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",29219,"ST",1,"LVM",1520,1,"1LE55033AA734GC6"]
["1LE5504-3AA73-4JA6","SIMOTICS SD MOTOR TYPE: 1CV4317A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F), according to 130(B) cast iron frame Basic Line Premium Efficiency IE4 2-pole * Size 315L* 315LkW (50 Hz) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * Flange: FF740 (A800) without motor protection Terminal box on left-hand side",32437,"ST",1,"LVM",1520,1,"1LE55043AA734JA6"]
["1LE5504-3AB73-4JC6","SIMOTICS SD MOTOR TYPE: 1CV4317B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F), according to 130(B) cast iron frame Basic Line Premium Efficiency IE4 4-pole * Size 315L* 315LkW (50 Hz) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * Flange: FF740 (A800) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",30748,"ST",1,"LVM",1560,1,"1LE55043AB734JC6"]
["1LE5603-3AA63-4JC6","SIMOTICS SD MOTOR TYPE: 1CV3316A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F), according to 130(B) cast iron frame Performance Line Premium Efficiency IE3, 2-pole * Size 315L* 250 kW (50 Hz) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 35 * Flange: FF740 (A800) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",24154,"ST",1,"LVM",1310,1,"1LE56033AA634JC6"]
["1LE5603-3AB63-4AC5","SIMOTICS SD MOTOR TYPE: 1CV3316B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F), according to 130(B) cast iron frame Performance Line Premium Efficiency IE3, 4-pole * Size 315L* 250 kW (50 Hz) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",22180,"ST",1,"LVM",1290,1,"1LE56033AB634AC5"]
["1LE5603-3BA43-4FB5","SIMOTICS SD MOTOR TYPE: 1CV3354A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F), according to 130(B) cast iron frame Performance Line Premium Efficiency IE3, 2-pole * Size 355L* 400 kW (50 Hz) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, Flange: FF840 (A900) disconnection (2 terminals) Terminal box on RHS",39619,"ST",1,"LVM",2240,1,"1LE56033BA434FB5"]
["1LE5603-3BB33-3AB6","SIMOTICS SD MOTOR TYPE: 1CV3353B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F), according to 130(B) cast iron frame Performance Line Premium Efficiency IE3, 4-pole * Size 355L* 355LkW (50 Hz) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 3, disconnection (2 terminals) Terminal box on left-hand side",31400,"ST",1,"LVM",2020,1,"1LE56033BB333AB6"]
["1LE5604-3AA63-3FB6","SIMOTICS SD MOTOR TYPE: 1CV4316A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F), according to 130(B) cast iron frame Performance Line Premium Efficiency IE4 2-pole * Size 315L* 250 kW (50 Hz) 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 5, Flange: FF740 (A800) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",26793,"ST",1,"LVM",1340,1,"1LE56043AA633FB6"]
["1LE5604-3AB73-4GB0","SIMOTICS SD MOTOR TYPE: 1CV4317B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F), according to 130(B) cast iron frame Performance Line Premium Efficiency IE4 4-pole * Size 315L* 315LkW (50 Hz) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1, Flange: FF740 (A800) 3 PTC thermistors for disconnection (2 terminals) Terminal box base left with terminal box at top",31328,"ST",1,"LVM",1560,1,"1LE56043AB734GB0"]
["1LE5604-3BA53-4AB6","SIMOTICS SD MOTOR TYPE: 1CV4355A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F), according to 130(B) cast iron frame Performance Line Premium Efficiency IE4 2-pole * Size 355L* 500 kW (50 Hz) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, disconnection (2 terminals) Terminal box on left-hand side",55705,"ST",1,"LVM",2340,1,"1LE56043BA534AB6"]
["1LE5604-3BB33-4FB6","SIMOTICS SD MOTOR TYPE: 1CV4353B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F), according to 130(B) cast iron frame Performance Line Premium Efficiency IE4 4-pole * Size 355L* 355LkW (50 Hz) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, Flange: FF840 (A900) disconnection (2 terminals) Terminal box on left-hand side",36679,"ST",1,"LVM",2050,1,"1LE56043BB334FB6"]
["1MB1011-0EA42-2HA4","SIMOTICS XP Motor type: 1AV2094A Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP65 temperature class 155(F) according to 130(B) Aluminum housing High Efficiency IE2 2-pole * Size 90L * 2.2kW (50 Hz) 2.55 (60 Hz) Version for Zone 21 and Zone 22 with conductive dust 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V3, flange: FF165 (A200) without motor protection Terminal box at top",506,"ST",1,"LVM",15,1,"1MB10110EA422HA4"]
["1MB1011-0EB42-2FA4","SIMOTICS XP Motor type: 1AV2094B Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP65 temperature class 155(F) according to 130(B) Aluminum housing High Efficiency IE2 4-pole * Size 90L * 1.5kW (50 Hz) 1.75 kW (60 Hz) Version for Zone 21 and Zone 22 with conductive dust 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B5, flange: FF165 (A200) without motor protection Terminal box at top",466,"ST",1,"LVM",16,1,"1MB10110EB422FA4"]
["1MB1011-1CA03-4HA4","SIMOTICS XP Motor type: 1AV2130A Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP65 temperature class 155(F) according to 130(B) Aluminum housing High Efficiency IE2 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) Version for Zone 21 and Zone 22 with conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V3, flange: FF265 (A300) without motor protection Terminal box at top",889,"ST",1,"LVM",44,1,"1MB10111CA034HA4"]
["1MB1011-1CC23-4HB4","SIMOTICS XP Motor type: 1AV2132C Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP65 temperature class 155(F) according to 130(B) Aluminum housing High Efficiency IE2 6-pole * Size 132M, * 4kW (50 Hz) 4.55 kW (60 Hz) Version for Zone 21 and Zone 22 with conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V3, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1089,"ST",1,"LVM",48,1,"1MB10111CC234HB4"]
["1MB1013-0DB33-4FA4","SIMOTICS XP Motor type: 1AV3083B Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP65 temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3 4-pole * Size 80M * 0.75kW (50 Hz) 0.86kW (60 Hz) Version for Zone 21 and Zone 22 with conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF165 (A200) without motor protection Terminal box at top",399,"ST",1,"LVM",14,1,"1MB10130DB334FA4"]
["1MB1013-0EB42-2FB4","SIMOTICS XP Motor type: 1AV3094B Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP65 temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3 4-pole * Size 90L * 1.5kW (50 Hz) 1.75 kW (60 Hz) Version for Zone 21 and Zone 22 with conductive dust 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B5, flange: FF165 (A200) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",551,"ST",1,"LVM",19,1,"1MB10130EB422FB4"]
["1MB1013-1CA02-2AB4","SIMOTICS XP Motor type: 1AV3130A Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP65 temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) Version for Zone 21 and Zone 22 with conductive dust 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",993,"ST",1,"LVM",43,1,"1MB10131CA022AB4"]
["1MB1013-1CB22-2FA4","SIMOTICS XP Motor type: 1AV3132B Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP65 temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3 4-pole * Size 132M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) Version for Zone 21 and Zone 22 with conductive dust 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B5, flange: FF265 (A300) without motor protection Terminal box at top",1257,"ST",1,"LVM",69,1,"1MB10131CB222FA4"]
["1MB1013-1DC42-2FA4","SIMOTICS XP Motor type: 1AV3164C Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP65 temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3 6-pole * Size 160L, * 11kW (50 Hz) 12.6kW (60 Hz) Version for Zone 21 and Zone 22 with conductive dust 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B5, flange: FF300 (A350) without motor protection Terminal box at top",2286,"ST",1,"LVM",124,1,"1MB10131DC422FA4"]
["1MB1021-0DA22-2HB4","SIMOTICS XP Motor type: 1AV2082A Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) Aluminum housing High Efficiency IE2 2-pole * Size 80M * 0.75kW (50 Hz) 0.86kW (60 Hz) Version for Zone 22 for non-conductive dust 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V3, flange: FF165 (A200) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",302,"ST",1,"LVM",9,1,"1MB10210DA222HB4"]
["1MB1021-0EB42-2HB4","SIMOTICS XP Motor type: 1AV2094B Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) Aluminum housing High Efficiency IE2 4-pole * Size 90L * 1.5kW (50 Hz) 1.75 kW (60 Hz) Version for Zone 22 for non-conductive dust 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V3, flange: FF165 (A200) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",435,"ST",1,"LVM",16,1,"1MB10210EB422HB4"]
["1MB1021-1CA03-4HA4","SIMOTICS XP Motor type: 1AV2130A Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) Aluminum housing High Efficiency IE2 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) Version for Zone 22 for non-conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V3, flange: FF265 (A300) without motor protection Terminal box at top",832,"ST",1,"LVM",44,1,"1MB10211CA034HA4"]
["1MB1021-1CC02-2FA4","SIMOTICS XP Motor type: 1AV2130C Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) Aluminum housing High Efficiency IE2 6-pole * Size 132S, * 3kW (50 Hz) 3.45kW (60 Hz) Version for Zone 22 for non-conductive dust 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B5, flange: FF265 (A300) without motor protection Terminal box at top",802,"ST",1,"LVM",43,1,"1MB10211CC022FA4"]
["1MB1021-1DC42-2AB4","SIMOTICS XP Motor type: 1AV2164C Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) Aluminum housing High Efficiency IE2 6-pole * Size 160L, * 11kW (50 Hz) 12.6kW (60 Hz) Version for Zone 22 for non-conductive dust 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1996,"ST",1,"LVM",93,1,"1MB10211DC422AB4"]
["1MB1023-0EA03-4FA4","SIMOTICS XP Motor type: 1AV3090A Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3 2-pole * Size 90S * 1.5kW (50 Hz) 1.75 kW (60 Hz) Version for Zone 22 for non-conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF165 (A200) without motor protection Terminal box at top",429,"ST",1,"LVM",15,1,"1MB10230EA034FA4"]
["1MB1023-1BB23-4FB4","SIMOTICS XP Motor type: 1AV3112B Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3 4-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) Version for Zone 22 for non-conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",822,"ST",1,"LVM",35,1,"1MB10231BB234FB4"]
["1MB1023-1CB02-2HA4","SIMOTICS XP Motor type: 1AV3130B Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3 4-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) Version for Zone 22 for non-conductive dust 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V3, flange: FF265 (A300) without motor protection Terminal box at top",977,"ST",1,"LVM",69,1,"1MB10231CB022HA4"]
["1MB1023-1DC43-4FB4","SIMOTICS XP Motor type: 1AV3164C Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3 6-pole * Size 160L, * 11kW (50 Hz) 12.6kW (60 Hz) Version for Zone 22 for non-conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2288,"ST",1,"LVM",124,1,"1MB10231DC434FB4"]
["1MB1031-0EA03-4HA4","SIMOTICS XP Motor type: 1AV2090A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2 2-pole * Size 90S * 1.5 kW (50 Hz) 1.75 kW (60 Hz) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V3, flange: FF165 (A200) without motor protection Terminal box at top",392,"ST",1,"LVM",13,1,"1MB10310EA034HA4"]
["1MB1031-1BA22-2FB4","SIMOTICS XP Motor type: 1AV2112A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2 2-pole * Size 112M, * 4 kW (50 Hz) 4.55 kW (60 Hz) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B5, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",730,"ST",1,"LVM",28,1,"1MB10311BA222FB4"]
["1MB1031-1BC23-4FA4","SIMOTICS XP Motor type: 1AV2112C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2 6-pole * Size 112M, * 2.2 kW (50 Hz) 2.55 kW (60 Hz) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF215 (A250) without motor protection Terminal box at top",657,"ST",1,"LVM",30,1,"1MB10311BC234FA4"]
["1MB1031-1CC03-4FB4","SIMOTICS XP Motor type: 1AV2130C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2 6-pole * Size 132S, * 3 kW (50 Hz) 3.45 kW (60 Hz) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",918,"ST",1,"LVM",43,1,"1MB10311CC034FB4"]
["1MB1033-0DA23-4HA4","SIMOTICS XP Motor type: 1AV3082A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing Premium Efficiency IE3 2-pole * Size 80M * 0.75 kW (50 Hz) 0.86 kW (60 Hz) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V3, flange: FF165 (A200) without motor protection Terminal box at top",353,"ST",1,"LVM",11,1,"1MB10330DA234HA4"]
["1MB1033-0EC42-2FA4","SIMOTICS XP Motor type: 1AV3094C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing Premium Efficiency IE3 6-pole * Size 90L * 1.1 kW (50 Hz) 1.27 kW (60 Hz) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B5, flange: FF165 (A200) without motor protection Terminal box at top",510,"ST",1,"LVM",19,1,"1MB10330EC422FA4"]
["1MB1033-1AB53-4AB4","SIMOTICS XP Motor type: 1AV3105B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing Premium Efficiency IE3 4-pole * Size 100L * 3 kW (50 Hz) 3.45 kW (60 Hz) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",669,"ST",1,"LVM",30,1,"1MB10331AB534AB4"]
["1MB1033-1DA23-4FB4","SIMOTICS XP Motor type: 1AV3162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing Premium Efficiency IE3 2-pole * Size 160M, * 11 kW (50 Hz) 12.6 kW (60 Hz) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1666,"ST",1,"LVM",84,1,"1MB10331DA234FB4"]
["1MB1033-1DC43-4FB4","SIMOTICS XP Motor type: 1AV3164C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing Premium Efficiency IE3 6-pole * Size 160L, * 11 kW (50 Hz) 12.6 kW (60 Hz) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2323,"ST",1,"LVM",124,1,"1MB10331DC434FB4"]
["1MB1511-0DB32-2HB4","SIMOTICS XP Motor type: 1CV2083B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP65 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 4-pole *Size 80M * 0.75 kW (1500 rpm) EX TB IIIC T120Β°DB Version for Zone 21 and Zone 22 with conductive dust 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM V 3, flange: FF165 (A200) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",421,"ST",1,"LVM",18.5,1,"1MB15110DB322HB4"]
["1MB1511-1AB52-2FA4","SIMOTICS XP Motor type: 1CV2105B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP65 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2 4-pole * Size 100L * 3 kW (50 Hz) 3.45 kW (60 Hz) EX TB IIIC T120Β°DB Version for Zone 21 and Zone 22 with conductive dust 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM B5, flange: FF215 (A250) without motor protection Terminal box at top",662,"ST",1,"LVM",37,1,"1MB15111AB522FA4"]
["1MB1511-1CB02-2HB4","SIMOTICS XP Motor type: 1CV2130B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP65 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2 4-pole * Size 132S, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) EX TB IIIC T120Β°DB Version for Zone 21 and Zone 22 with conductive dust 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM V3, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1080,"ST",1,"LVM",61,1,"1MB15111CB022HB4"]
["1MB1511-1DB42-2FB4","SIMOTICS XP Motor type: 1CV2164B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP65 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2 4-pole * Size 160L, * 15 kW (50 Hz) 17.3 kW (60 Hz) EX TB IIIC T120Β°DB Version for Zone 21 and Zone 22 with conductive dust 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM B5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2082,"ST",1,"LVM",104,1,"1MB15111DB422FB4"]
["1MB1511-1DB23-4FB4","SIMOTICS XP Motor type: 1CV2162B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP65 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2 4-pole * Size 160M, * 11 kW (50 Hz) 12.6 kW (60 Hz) EX TB IIIC T120Β°DB Version for Zone 21 and Zone 22 with conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1688,"ST",1,"LVM",96,1,"1MB15111DB234FB4"]
["1MB1513-1AB53-4FB4","SIMOTICS XP Motor type: 1CV3105B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP65 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3 4-pole * Size 100L * 3 kW (50 Hz) 3.45 kW (60 Hz) EX TB IIIC T120Β°DB Version for Zone 21 and Zone 22 with conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",783,"ST",1,"LVM",40,1,"1MB15131AB534FB4"]
["1MB1513-1BB22-2FA4","SIMOTICS XP Motor type: 1CV3112B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP65 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3 4-pole * Size 112M, * 4 kW (50 Hz) 4.55 kW (60 Hz) EX TB IIIC T120Β°DB Version for Zone 21 and Zone 22 with conductive dust 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM B5, flange: FF215 (A250) without motor protection Terminal box at top",880,"ST",1,"LVM",46,1,"1MB15131BB222FA4"]
["1MB1513-1CC02-2AB4","SIMOTICS XP Motor type: 1CV3130C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP65 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3 6-pole * Size 132S, * 3 kW (50 Hz) 3.45 kW (60 Hz) EX TB IIIC T120Β°DB Version for Zone 21 and Zone 22 with conductive dust 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1028,"ST",1,"LVM",70,1,"1MB15131CC022AB4"]
["1MB1521-0DA22-2FA4","SIMOTICS XP Motor type: 1CV2082A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 2-pole *Size 80M * 0.75 kW (3000 rpm) EX TC IIIB T120Β° DC Version for Zone 22 for non-conductive dust 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM B 5, flange: FF165 (A200) without motor protection Terminal box at top",334,"ST",1,"LVM",16,1,"1MB15210DA222FA4"]
["1MB1521-0DC23-4HA4","SIMOTICS XP Motor type: 1CV2082C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 6-pole *Size 80M * 0.37 kW (1000 rpm) EX TC IIIB T120Β° DC Version for Zone 22 for non-conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 3, flange: FF165 (A200) without motor protection Terminal box at top",324,"ST",1,"LVM",16.5,1,"1MB15210DC234HA4"]
["1MB1521-1BB23-4AB4","SIMOTICS XP Motor type: 1CV2112B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2 4-pole * Size 112M, * 4 kW (50 Hz) 4.55 kW (60 Hz) EX TC IIIB T120Β° DC Version for Zone 22 for non-conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",753,"ST",1,"LVM",46,1,"1MB15211BB234AB4"]
["1MB1521-1DA33-4FA4","SIMOTICS XP Motor type: 1CV2163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2 2-pole * Size 160M, * 15 kW (50 Hz) 17.3 kW (60 Hz) EX TC IIIB T120Β° DC Version for Zone 22 for non-conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF300 (A350) without motor protection Terminal box at top",1909,"ST",1,"LVM",104,1,"1MB15211DA334FA4"]
["1MB1523-0DA32-2FB4","SIMOTICS XP Motor type: 1CV3083A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE3, 2-pole *Size 80M * 1.1 kW (3000 rpm) EX TC IIIB T120Β° DC Version for Zone 22 for non-conductive dust 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM B 5, flange: FF165 (A200) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",469,"ST",1,"LVM",21,1,"1MB15230DA322FB4"]
["1MB1523-0DC33-4AB4","SIMOTICS XP Motor type: 1CV3083C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE3, 6-pole *Size 80M * 0.55 kW (1000 rpm) EX TC IIIB T120Β° DC Version for Zone 22 for non-conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",435,"ST",1,"LVM",22.5,1,"1MB15230DC334AB4"]
["1MB1523-1BA22-2AB4","SIMOTICS XP Motor type: 1CV3112A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3 2-pole * Size 112M, * 4 kW (50 Hz) 4.55 kW (60 Hz) EX TC IIIB T120Β° DC Version for Zone 22 for non-conductive dust 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",779,"ST",1,"LVM",45,1,"1MB15231BA222AB4"]
["1MB1523-1CA13-4FA4","SIMOTICS XP Motor type: 1CV3131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3 2-pole * Size 132S, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) EX TC IIIB T120Β° DC Version for Zone 22 for non-conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF265 (A300) without motor protection Terminal box at top",1213,"ST",1,"LVM",73,1,"1MB15231CA134FA4"]
["1MB1523-1DC43-4FB4","SIMOTICS XP Motor type: 1CV3164C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3 6-pole * Size 160L, * 11 kW (50 Hz) 12.6 kW (60 Hz) EX TC IIIB T120Β° DC Version for Zone 22 for non-conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2468,"ST",1,"LVM",147,1,"1MB15231DC434FB4"]
["1MB1531-0DC33-4FB4","SIMOTICS XP Motor type: 1CV2083C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 6-pole *Size 80M * 0.55 kW (1000 rpm) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF165 (A200) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",405,"ST",1,"LVM",18.5,1,"1MB15310DC334FB4"]
["1MB1531-0EC03-4AA4","SIMOTICS XP Motor type: 1CV2090C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 6-pole *Size 90S * 0.75 kW (1000 rpm) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 without motor protection Terminal box at top",409,"ST",1,"LVM",23,1,"1MB15310EC034AA4"]
["1MB1531-1CA02-2FB4","SIMOTICS XP Motor type: 1CV2130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2 2-pole * Size 132S, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM B5, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",997,"ST",1,"LVM",57,1,"1MB15311CA022FB4"]
["1MB1533-0DA22-2FA4","SIMOTICS XP Motor type: 1CV3082A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE3, 2-pole *Size 80M * 0.75 kW (3000 rpm) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM B 5, flange: FF165 (A200) without motor protection Terminal box at top",426,"ST",1,"LVM",18,1,"1MB15330DA222FA4"]
["1MB1533-0DA22-2FB4","SIMOTICS XP Motor type: 1CV3082A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE3, 2-pole *Size 80M * 0.75 kW (3000 rpm) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM B 5, flange: FF165 (A200) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",443,"ST",1,"LVM",18,1,"1MB15330DA222FB4"]
["1MB1533-1AB53-4FB4","SIMOTICS XP Motor type: 1CV3105B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3 4-pole * Size 100L * 3 kW (50 Hz) 3.45 kW (60 Hz) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",757,"ST",1,"LVM",40,1,"1MB15331AB534FB4"]
["1MB1533-1CA12-2AA4","SIMOTICS XP Motor type: 1CV3131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3 2-pole * Size 132S, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM B3 without motor protection Terminal box at top",1187,"ST",1,"LVM",73,1,"1MB15331CA122AA4"]
["1MB1533-1DB42-2FB4","SIMOTICS XP Motor type: 1CV3164B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3 4-pole * Size 160L, * 15 kW (50 Hz) 17.3 kW (60 Hz) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM B5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2258,"ST",1,"LVM",127,1,"1MB15331DB422FB4"]
["1MB2121-1CB31-4EG3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR HAZARDOUS DUTY XP100 CAST-IRON HOUSING NP EFFICIENCY, TEFC (IP65) 4 POLE * FS 184T 5 HP (60 HZ) CLASS I, GROUPS C&D, DIVISION I CLASS II,GROUPS F&G, DIVISION I 230/460V, 60HZ (SUITABLE FOR 208V) C-FACE WITH FEET C-1,2; F-1,2; W -1...8 thermostat FLOOR F-1",1642,"ST",1,"LVM",56.7,1,"1MB21211CB314EG3"]
["1MB2121-3CC21-3AG3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR HAZARDOUS DUTY XP100 CAST-IRON HOUSING NP EFFICIENCY, TEFC (IP65) 6 POLE * FS 365T 50 HP (60 HZ) CLASS I, GROUPS C&D, DIVISION I CLASS II,GROUPS F&G, DIVISION I 575V STD, 60HZ FOOT MOUNTED F-1,2 thermostat FLOOR F-1",12087,"ST",1,"LVM",394.63200000000001,1,"1MB21213CC213AG3"]
["1MB2121-4CB61-2AG3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR HAZARDOUS DUTY XP100 CAST-IRON HOUSING NP EFFICIENCY, TEFC (IP65) 4 POLE * FS 449T 300 HP (60HZ) CLASS I, GROUPS C&D, DIVISION I CLASS II,GROUPS F&G, DIVISION I BEARING DESIGN FOR INCREASED CANTILEVER FORCES 460V, 60HZ FOOT MOUNTED F-1,2 THERMOSTATS, KLIXON, NORMALLY CLOSED FLOOR F-1",45450,"ST",1,"LVM",1065.96,1,"1MB21214CB612AG3"]
["1MB2221-3AC21-6AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR HAZARDOUS DUTY XP100 ID1 CAST-IRON HOUSING NP EFFICIENCY, TEFC (IP65) 6 POLE *  FS 326T 30 HP (60 HZ) CLASS I, GROUP D, DIVISION I 230/460V STD 60HZ FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",6965,"ST",1,"LVM",307.541,1,"1MB22213AC216AA3"]
["1MB2221-4EC31-2AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR HAZARDOUS DUTY XP100 ID1 CAST-IRON HOUSING NP EFFICIENCY, TEFC (IP65) 6 POLE *  FS B447T 150 HP (60 HZ) CLASS I, GROUP D, DIVISION I 460V STD, 60HZ FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",25323,"ST",1,"LVM",903.11800000000005,1,"1MB22214EC312AA3"]
["3DX4100-0B","crank for auxiliary operating mechanism","On Request","ST",1,"LP",0.5,0,"3DX41000B"]
["3KA7121-4BD02","Change-over switch 4 x 160 A over- lap-WI",3707,"ST",null,"LP",6,1,"3KA71214BD02"]
["3KA7132-3AA00","SECTION 3x 400 A SANS COMM",382,"ST",null,"LP",3,1,"3KA71323AA00"]
["3KA7153-4BD01","INVERSOR DE REDE MOTORIZADO,",8081,"ST",null,"LP",1,1,"3KA71534BD01"]
["3KA7157-4DD00","Change-over switch 4 x 3150 A horizontal",21911,"ST",null,"LP",74,1,"3KA71574DD00"]
["3KC4342-0DA21-0AA3","SENTRON, transfer switching equipment 3KC, remotely operated, RTSE, 3-pole, Iu: 400 A, Ue AC: 415 V, Ie at AC-33 B at 415 V: 200 A, Ie at AC-23 A at 690 V: 125 A, screw mounting, motorized operating mechanism, at the right end, long handle, busbar connection",2065,"ST",null,"LP",9.24,1,"3KC43420DA210AA3"]
["3KD2830-0NE10-0","Switch disconnector 80 A, Size 2, 3-pole Front operating mechanism left Basic unit without handle flat terminal incl. phase barriers",61.8,"ST",null,"LP",1.0489999999999999,1,"3KD28300NE100"]
["3KD3832-0PE10-0","Switch disconnector 250 A, Size 3, 3-pole Front operating mechanism left Complete unit with direct operating mechanism gray flat terminal",265,"ST",null,"LP",2.98,1,"3KD38320PE100"]
["3KD4832-0QE10-0","Switch disconnector 800 A, Size 4, 3-pole Front operating mechanism left Complete unit with direct operating mechanism gray flat terminal",781,"ST",null,"LP",7.54,1,"3KD48320QE100"]
["3KD9415-2","Accessory for 3KD size 4 door-coupling rotary operating mechanism Complete operating mechanism, yellow/red incl. shaft 300 mm long and clutch holder Can be locked in OFF position",65.8,"ST",null,"LP",0.96399999999999997,1,"3KD94152"]
["3KE4330-0GA","switch disconnector, 3-pole with door op. mechanism 8UC7 handle dark gray/blue-green basic masking plate, light gray",1418,"ST",null,"LP",5.38,1,"3KE43300GA"]
["3KL7132-4AD00","SECTION FUS-NH 4x 250 A COMM MOT",4990,"ST",null,"LP",1,1,"3KL71324AD00"]
["3KL7142-4CA00","Switch disconnector with fuses 4x 400A W",858,"ST",null,"LP",7.5,1,"3KL71424CA00"]
["3KM5230-5AB01","Switch disconnector with fuse For rated current 125 A, 3-pole without operating mechanism, without shaft with lyra contacts in new design",449,"ST",null,"LP",2.3610000000000002,1,"3KM52305AB01"]
["3KX3536-3AA","Accessory for switch 3KL53 Assembly kit Rear-side manual operating mechanism can be locked black, including cover",246,"ST",null,"LP",0.88,1,"3KX35363AA"]
["3KX7122-5AA00","INTERRUPTEUR PAR horizontal Sz. 5 1250 A",390,"ST",null,"LP",2.4,1,"3KX71225AA00"]
["3KX7144-8AA00","AUXILIARY Contacts 4NA+4NC for 3K-718 SI",77.900000000000006,"ST",null,"LP",0.1,1,"3KX71448AA00"]
["3LD2003-1TL51","SENTRON, Switch disconnector 3LD, main switch, 4-pole, Iu: 16 A, Operating power / at AC-23 A at 400 V: 7.5 kW, front-mounted, rotary operating mechanism, black, 4-hole mounting of the handle",32.200000000000003,"ST",null,"LP",0.218,1,"3LD20031TL51"]
["3LD2154-2EP53","SENTRON, Switch disconnector 3LD, emergency switching-off switch, 4- pole, Iu: 25 A, operating power / at AC-23 A 400 V: 9.5 kW, front-mounted, 1 NC, 1 NO, rotary operating mechanism, Red / yellow, Central mounting 22.5 mm of the handle",42.7,"ST",null,"LP",0.26,1,"3LD21542EP53"]
["3LD2305-0TK11","SENTRON, Switch disconnector 3LD, main switch, 3-pole, Iu: 160 A, Operating power / at AC-23 A at 400 V: 75 kW, front-mounted, knob-operated mechanism, black, 4-hole mounting of the handle",269,"ST",null,"LP",2.089,1,"3LD23050TK11"]
["3LD2524-7UK01","SENTRON, Switch disconnector 3LD, change-over switch, 3-pole, Iu: 63 A, Operating power / at AC-23 A at 400 V: 22 kW, front-mounted, knob-operated mechanism, black, 4-hole mounting of the handle",102,"ST",null,"LP",0.72899999999999998,1,"3LD25247UK01"]
["3LD2766-0TB53-0US2","SENTRON, Switch disconnector 3LD, emergency switching-off switch, 3- pole, Iu: 100 A, operating power / at AC-23 A 400 V: 37 kW, Molded plastic encapsulation for inch cable gland, rotary operating mechanism, red/yellow",274,"ST",null,"LP",1.8979999999999999,1,"3LD27660TB530US2"]
["3NA3132","LV HRC fuse element, NH1, In: 125 A, gG, Un AC: 500 V, Un DC: 440 V, Front indicator, live grip lugs",9.8699999999999992,"ST",null,"LP",0.28899999999999998,3,"3NA3132"]
["3NA3344","LV HRC fuse element, NH3, In: 250 A, gG, Un AC: 500 V, Un DC: 440 V, Front indicator, live grip lugs",24.5,"ST",null,"LP",0.65600000000000003,3,"3NA3344"]
["3NA6140","LV HRC fuse element, NH1, In: 200 A, gG, Un AC: 500 V, Un DC: 440 V, Combined indicator, Insulated grip lugs",17.600000000000001,"ST",null,"LP",0.44700000000000001,3,"3NA6140"]
["3NA6824-4KK","LV HRC fuse element, NH00, In: 80 A, gG, Un AC: 400 V, Combined indicator, insulated Grip lugs",8.2799999999999994,"ST",null,"LP",0.20100000000000001,3,"3NA68244KK"]
["3NC1003","SITOR cylindrical fuse link, 10 x 38 mm, 3 A, aR, Un AC: 600 V, Un DC: 700 V, DC according to UL",18.5,"ST",null,"LP",8.9999999999999993E-3,10,"3NC1003"]
["3NC2240","SITOR cylindrical fuse link, 22x58 mm, 40 A, aR, Un AC: 690 V, Un DC: 700 V, DC according to UL",15.2,"ST",null,"LP",5.7000000000000002E-2,5,"3NC2240"]
["3NE1220-5E","PV fuse link, with blade contacts, NH1XL, In: 80 A, gPV, Un DC: 1500 V, front indicator",322,"ST",null,"LP",0.99399999999999999,2,"3NE12205E"]
["3NE1447-2","SITOR fuse link, with blade contacts, NH3, In: 670 A, gR, Un AC: 690 V, Un DC: 440 V, front indicator",339,"ST",null,"LP",1.1919999999999999,3,"3NE14472"]
["3NE8024-1","SITOR fuse link, with blade contacts, NH00, In: 160 A, aR, Un AC: 690 V, Un DC: 440 V, front indicator",57.1,"ST",null,"LP",0.20899999999999999,3,"3NE80241"]
["3NH3530","LV HRC fuse base Sz. 4, 1-pole 1250 A, 690 V flat terminal",188,"ST",null,"LP",3.1070000000000002,1,"3NH3530"]
["3NJ4911-2BQ00","Accessory for strips 3NJ41, Sz. NH1-3, Box terminal 95-240 mm2 consists of 3 box terminals",106,"ST",null,"LP",0.98,1,"3NJ49112BQ00"]
["3NJ6233-1AA00-0CL5","Switch disconnector with fuses In-line design, pluggable NH3 630 A, 3-pole Standard switching capacity S manual operation without auxiliary switch 3 current transformers for Multifunctional connector 600/5 A, Cl. 0.5","On Request","ST",null,"LP",15.36,1,"3NJ62331AA000CL5"]
["3NJ6930-3FE00","accessory for Switch disconnector with fuses In-line design, plug-in, NH1 Electronic fuse monitoring and line monitoring EFM 25, for DC networks",553,"ST",null,"LP",0.11,1,"3NJ69303FE00"]
["3NJ6940-3BJ23","accessory for Switch disconnector with fuses In-line design, pluggable current transformer 400/5 A, Cl. 0.5, legal-for-trade calibrated, 5 VA",625,"ST",null,"LP",0.35499999999999998,1,"3NJ69403BJ23"]
["3NP1133-1JB10","SENTRON, Fuse switch disconnector 3NP1, 3-pole, NH00, 160 A, for Rittal busbar system 40 mm, flat terminal, Cover level 32/70 mm",114,"ST",null,"LP",1.1259999999999999,1,"3NP11331JB10"]
["3NP1943-1BA00","Saddle terminal 70 - 150 mm2, for size NH1 with screw terminal, accessory for fuse switch disconnector 3NP1 Contains 3 terminals",17,"ST",null,"LP",0.13200000000000001,1,"3NP19431BA00"]
["3NP1963-1BA00","Saddle terminal 150 - 300 mm2, for size NH3 with screw terminal, accessory for fuse switch disconnector 3NP1 Contains 3 terminals",26.8,"ST",null,"LP",0.379,1,"3NP19631BA00"]
["3NW3080-0HG","SENTRON, cylindrical fuse link, Class CC, 8 A, time-lag, current-limiting, Un AC: 600 V, respect national installation rules!",33.5,"ST",null,"LP",8.0000000000000002E-3,10,"3NW30800HG"]
["3NW7151","SENTRON, cylindrical fuse holder, 14x51 mm, 1P+N, In: 50 A, Un AC: 690 V",40,"ST",null,"LP",0.23400000000000001,1,"3NW7151"]
["3NX2030","Phase/end barrier for LV HRC base Sz. 0",7.52,"ST",null,"LP",3.9E-2,2,"3NX2030"]
["3NY3035","Accessory for switch 3NP35/ 3NP4.7 and 3NP401 Auxiliary current switch 1 CO with screws (mounting kit)","On Request","ST",1,"LP",4.0000000000000001E-3,1,"3NY3035"]
["3VA1010-3ED32-0AE0","Circuit breaker 3VA1 IEC Frame 100 Switching capacity class N Icu=25 kA @ 415 V 3-pole, system protection TM210, FTFM, In=100 A Overload protection Ir=100 A non-adjustable short-circuit protection Ii = 10 x In Lug terminal 4 auxiliary switches HQ",215,"ST",null,"LP",1.02,1,"3VA10103ED320AE0"]
["3VA1010-3ED36-0CH0","Circuit breaker 3VA1 IEC Frame 100 Switching capacity class N Icu=25 kA @ 415 V 3-pole, system protection TM210, FTFM, In=100 A Overload protection Ir=100 A non-adjustable short-circuit protection Ii = 10 x In Terminal connection Undervoltage release (UVR) 120-127 V AC 50/60 Hz 2 auxiliary switches HQ 1 tripped signaling contact HQ",284,"ST",null,"LP",1.08,1,"3VA10103ED360CH0"]
["3VA1010-4ED36-0AE0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=100A overload protection Ir=100A fixed short-circuit protection Ii=10 x In clamp connection 4 auxiliary switches HQ",241,"ST",null,"LP",1.02,1,"3VA10104ED360AE0"]
["3VA1020-3ED32-0AF0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM210, FTFM, In=20A overload protection Ir=20A fixed short-circuit protection Ii=16 x In nut keeper kit 1 auxiliary switch HQ 1 trip alarm switch HQ",187,"ST",null,"LP",0.96,1,"3VA10203ED320AF0"]
["3VA1025-2ED32-0DH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 3-pole, line protection TM210, FTFM, In=25A overload protection Ir=25A fixed short-circuit protection Ii=12.8 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",289,"ST",null,"LP",1.08,1,"3VA10252ED320DH0"]
["3VA1025-4ED32-0DH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=25A overload protection Ir=25A fixed short-circuit protection Ii=12.8 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",295,"ST",null,"LP",1.08,1,"3VA10254ED320DH0"]
["3VA1032-2ED32-0JH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 3-pole, line protection TM210, FTFM, In=32A overload protection Ir=32A fixed short-circuit protection Ii=10 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",269,"ST",null,"LP",1.08,1,"3VA10322ED320JH0"]
["3VA1040-2ED32-0AD0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 3-pole, line protection TM210, FTFM, In=40A overload protection Ir=40A fixed short-circuit protection Ii=10 x In nut keeper kit 3 auxiliary switches HQ",203,"ST",null,"LP",0.99,1,"3VA10402ED320AD0"]
["3VA1040-3ED46-0AA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 4-pole, line protection TM210, FTFM, In=40A overload protection Ir=40A fixed short-circuit protection Ii=10 x In N conductor unprotected clamp connection",211,"ST",null,"LP",1.274,1,"3VA10403ED460AA0"]
["3VA1050-2ED36-0JA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 3-pole, line protection TM210, FTFM, In=50A overload protection Ir=50A fixed short-circuit protection Ii=10 x In clamp connection shunt trip (STL) 110-127V DC, AC 50/60Hz",231,"ST",null,"LP",1.05,1,"3VA10502ED360JA0"]
["3VA1050-3ED36-0AA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM210, FTFM, In=50A overload protection Ir=50A fixed short-circuit protection Ii=10 x In clamp connection",162,"ST",null,"LP",1.0249999999999999,1,"3VA10503ED360AA0"]
["3VA1050-4ED42-0DH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM210, FTFM, In=50A overload protection Ir=50A fixed short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",341,"ST",null,"LP",1.38,1,"3VA10504ED420DH0"]
["3VA1063-2ED32-0KC0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 3-pole, line protection TM210, FTFM, In=63A overload protection Ir=63A fixed short-circuit protection Ii=10 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ",249,"ST",null,"LP",1.05,1,"3VA10632ED320KC0"]
["3VA1063-3ED36-0AD0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM210, FTFM, In=63A overload protection Ir=63A fixed short-circuit protection Ii=10 x In clamp connection 3 auxiliary switches HQ",222,"ST",null,"LP",0.99,1,"3VA10633ED360AD0"]
["3VA1063-4ED36-0JA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=63A overload protection Ir=63A fixed short-circuit protection Ii=10 x In clamp connection shunt trip (STL) 110-127V DC, AC 50/60Hz",237,"ST",null,"LP",1.05,1,"3VA10634ED360JA0"]
["3VA1080-3ED36-0AH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM210, FTFM, In=80A overload protection Ir=80A fixed short-circuit protection Ii=10 x In clamp connection 2 auxiliary switches HQ 1 trip alarm switch HQ",216,"ST",null,"LP",0.99,1,"3VA10803ED360AH0"]
["3VA1080-3ED42-0DH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 4-pole, line protection TM210, FTFM, In=80A overload protection Ir=80A fixed short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",322,"ST",null,"LP",1.38,1,"3VA10803ED420DH0"]
["3VA1096-2ED42-0AA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 4-pole, line protection TM210, FTFM, In=16A overload protection Ir=16A fixed short-circuit protection Ii=20 x In N conductor unprotected nut keeper kit",185,"ST",null,"LP",1.2,1,"3VA10962ED420AA0"]
["3VA1104-5MG36-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, starter protection TM110M, FM, In=4A without overload protection short-circuit protection Ii=15 x In clamp connection",204,"ST",null,"LP",1.0209999999999999,1,"3VA11045MG360AA0"]
["3VA1110-3EF32-0AF0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=5...10 x In nut keeper kit 1 auxiliary switch HQ 1 trip alarm switch HQ",195,"ST",null,"LP",0.96,1,"3VA11103EF320AF0"]
["3VA1110-3GD42-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 4-pole, line protection TM210, FTFM, In=100A overload protection Ir=100A fixed short-circuit protection Ii=10 x In N conductor protection 100% nut keeper kit",210,"ST",null,"LP",1.2090000000000001,1,"3VA11103GD420AA0"]
["3VA1110-4EF32-0CC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ",355,"ST",null,"LP",1.05,1,"3VA11104EF320CC0"]
["3VA1110-5EE32-0KA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM220, ATFM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=10 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC",269,"ST",null,"LP",1.05,1,"3VA11105EE320KA0"]
["3VA1110-5EF36-0JH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=5...10 x In clamp connection shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",517,"ST",null,"LP",1.08,1,"3VA11105EF360JH0"]
["3VA1110-5MH36-0KC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, starter protection TM120M, AM, In=100A without overload protection short-circuit protection Ii=5...15 x In clamp connection shunt trip (STL) 220-250 V DC; 208-277 V AC 2 auxiliary switches HQ",352,"ST",null,"LP",1.05,1,"3VA11105MH360KC0"]
["3VA1110-6GF42-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 4-pole, line protection TM240, ATAM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=5...10 x In N conductor protection 100% nut keeper kit",338,"ST",null,"LP",1.228,1,"3VA11106GF420AA0"]
["3VA1112-1AA42-0KC0","switch disconnector 3VA1 IEC frame 160 4-pole SD100, In=125A without overload protection w/o short-circuit protection nut keeper kit shunt trip (STL) 220-250V DC; 208-277V AC 2 auxiliary switches HQ",371,"ST",null,"LP",1.35,1,"3VA11121AA420KC0"]
["3VA1112-3EF32-0HA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=125A overload protection Ir=88A...125A short-circuit protection Ii=5...10 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz",319,"ST",null,"LP",0.9,1,"3VA11123EF320HA0"]
["3VA1112-5ED32-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM210, FTFM, In=125A overload protection Ir=125A fixed short-circuit protection Ii=10 x In nut keeper kit",346,"ST",null,"LP",1.02,1,"3VA11125ED320AA0"]
["3VA1112-5EF32-0HH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=125A overload protection Ir=88A...125A short-circuit protection Ii=5...10 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",433,"ST",null,"LP",1.08,1,"3VA11125EF320HH0"]
["3VA1112-5MH36-0HA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, starter protection TM120M, AM, In=125A without overload protection short-circuit protection Ii=5...15 x In clamp connection shunt trip (STL) 12-30 V DC; 24 V AC 50/60 Hz",463,"ST",null,"LP",0.9,1,"3VA11125MH360HA0"]
["3VA1112-6EF36-0CC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=125A overload protection Ir=88A...125A short-circuit protection Ii=5...10 x In clamp connection undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ",424,"ST",null,"LP",1.05,1,"3VA11126EF360CC0"]
["3VA1116-1AA36-0AE0","switch disconnector 3VA1 IEC frame 160 3-pole SD100, In=160A without overload protection w/o short-circuit protection clamp connection 4 auxiliary switches HQ",311,"ST",null,"LP",1.02,1,"3VA11161AA360AE0"]
["3VA1116-3ED22-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 2-pole, line protection TM210, FTFM, In=160A overload protection Ir=160A fixed short-circuit protection Ii=10 x In nut keeper kit",252,"ST",null,"LP",0.67800000000000005,1,"3VA11163ED220AA0"]
["3VA1116-4EF32-0JC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",371,"ST",null,"LP",1.05,1,"3VA11164EF320JC0"]
["3VA1116-4EF46-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In N conductor unprotected clamp connection",405,"ST",null,"LP",1.333,1,"3VA11164EF460AA0"]
["3VA1116-5EE32-0BA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM220, ATFM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=10 x In nut keeper kit undervoltage release (UVR) 24V DC",372,"ST",null,"LP",0.9,1,"3VA11165EE320BA0"]
["3VA1116-5FF46-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In N conductor protection 50% clamp connection",503,"ST",null,"LP",1.17,1,"3VA11165FF460AA0"]
["3VA1120-3EF32-0BC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=20A overload protection Ir=14A...20A short-circuit protection Ii=8...16 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ",282,"ST",null,"LP",1.05,1,"3VA11203EF320BC0"]
["3VA1120-3EF36-0JH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=20A overload protection Ir=14A...20A short-circuit protection Ii=8...16 x In clamp connection shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",297,"ST",null,"LP",1.08,1,"3VA11203EF360JH0"]
["3VA1120-4EF36-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=20A overload protection Ir=14A...20A short-circuit protection Ii=8...16 x In clamp connection",231,"ST",null,"LP",1.034,1,"3VA11204EF360AA0"]
["3VA1120-6EF32-0DH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=20A overload protection Ir=14A...20A short-circuit protection Ii=8...16 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",585,"ST",null,"LP",1.08,1,"3VA11206EF320DH0"]
["3VA1120-6EF36-0KA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=20A overload protection Ir=14A...20A short-circuit protection Ii=8...16 x In clamp connection shunt trip (STL) 220-250V DC, 208-277V AC",492,"ST",null,"LP",1.05,1,"3VA11206EF360KA0"]
["3VA1125-5ED22-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 2-pole, line protection TM210, FTFM, In=25A overload protection Ir=25A fixed short-circuit protection Ii=12.8 x In nut keeper kit",180,"ST",null,"LP",0.65100000000000002,1,"3VA11255ED220AA0"]
["3VA1125-5EF36-0DC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=25A overload protection Ir=18A...25A short-circuit protection Ii=6.4...12.8 x In clamp connection undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",564,"ST",null,"LP",1.05,1,"3VA11255EF360DC0"]
["3VA1132-3EF36-0KC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=32A overload protection Ir=22A...32A short-circuit protection Ii=5...10 x In clamp connection shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ",279,"ST",null,"LP",1.05,1,"3VA11323EF360KC0"]
["3VA1132-4ED46-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM210, FTFM, In=32A overload protection Ir=32A fixed short-circuit protection Ii=10 x In N conductor unprotected clamp connection",259,"ST",null,"LP",1.17,1,"3VA11324ED460AA0"]
["3VA1132-5GD42-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM210, FTFM, In=32A overload protection Ir=32A fixed short-circuit protection Ii=10 x In N conductor protection 100% nut keeper kit",227,"ST",null,"LP",1.2,1,"3VA11325GD420AA0"]
["3VA1132-6EF32-0DA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=32A overload protection Ir=22A...32A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz",495,"ST",null,"LP",0.9,1,"3VA11326EF320DA0"]
["3VA1140-4EE42-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM220, ATFM, In=40A overload protection Ir=28A...40A short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit",182,"ST",null,"LP",1.1870000000000001,1,"3VA11404EE420AA0"]
["3VA1140-4EF36-0AC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=40A overload protection Ir=28A...40A short-circuit protection Ii=5...10 x In clamp connection 2 auxiliary switches HQ",274,"ST",null,"LP",0.96,1,"3VA11404EF360AC0"]
["3VA1140-6EE36-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM220, ATFM, In=40A overload protection Ir=28A...40A short-circuit protection Ii=10 x In clamp connection",267,"ST",null,"LP",1.028,1,"3VA11406EE360AA0"]
["3VA1140-6EF42-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 4-pole, line protection TM240, ATAM, In=40A overload protection Ir=28A...40A short-circuit protection Ii=5...10 x In N conductor unprotected nut keeper kit",462,"ST",null,"LP",1.2,1,"3VA11406EF420AA0"]
["3VA1150-4EF32-0DH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=50A overload protection Ir=35A...50A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",374,"ST",null,"LP",1.08,1,"3VA11504EF320DH0"]
["3VA1150-5EE36-0AC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM220, ATFM, In=50A overload protection Ir=35A...50A short-circuit protection Ii=10 x In clamp connection circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 2 auxiliary switches HQ",181,"ST",null,"LP",1.07,1,"3VA11505EE360AC0"]
["3VA1150-6EF32-0HC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=50A overload protection Ir=35A...50A short-circuit protection Ii=5...10 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ",523,"ST",null,"LP",1.05,1,"3VA11506EF320HC0"]
["3VA1163-1AA32-0BC0","switch disconnector 3VA1 IEC frame 160 3-pole SD100, In=63A without overload protection w/o short-circuit protection nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ",244,"ST",null,"LP",1.05,1,"3VA11631AA320BC0"]
["3VA1163-1AA42-0CC0","switch disconnector 3VA1 IEC frame 160 4-pole SD100, In=63A without overload protection w/o short-circuit protection nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ",283,"ST",null,"LP",1.35,1,"3VA11631AA420CC0"]
["3VA1163-4EF32-0BH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=63A overload protection Ir=44A...63A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ",374,"ST",null,"LP",1.05,1,"3VA11634EF320BH0"]
["3VA1163-4EF36-0HA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=63A overload protection Ir=44A...63A short-circuit protection Ii=5...10 x In clamp connection shunt trip (STL) 12-30V DC, 24V AC 50/60Hz",309,"ST",null,"LP",0.9,1,"3VA11634EF360HA0"]
["3VA1163-5EF32-0DA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=63A overload protection Ir=44A...63A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz",475,"ST",null,"LP",0.9,1,"3VA11635EF320DA0"]
["3VA1163-5MH32-0KH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, starter protection TM120M, AM, In=63A without overload protection short-circuit protection Ii=5...15 x In nut keeper kit shunt trip (STL) 220-250 V DC; 208-277 V AC 2 auxiliary switches HQ 1 trip alarm switch HQ",294,"ST",null,"LP",1.08,1,"3VA11635MH320KH0"]
["3VA1163-6MH36-0CA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, starter protection TM120M, AM, In=63A without overload protection short-circuit protection Ii=5...15 x In clamp connection undervoltage release (UVR) 120-127V AC 50/60Hz",302,"ST",null,"LP",0.9,1,"3VA11636MH360CA0"]
["3VA1180-3EF32-0AB0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=80A overload protection Ir=56A...80A short-circuit protection Ii=5...10 x In nut keeper kit 2 auxiliary switches HP",210,"ST",null,"LP",0.96,1,"3VA11803EF320AB0"]
["3VA1180-4EF36-0CH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=80A overload protection Ir=56A...80A short-circuit protection Ii=5...10 x In clamp connection undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",381,"ST",null,"LP",1.08,1,"3VA11804EF360CH0"]
["3VA1180-5EF32-0JC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=80A overload protection Ir=56A...80A short-circuit protection Ii=5...10 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",425,"ST",null,"LP",1.05,1,"3VA11805EF320JC0"]
["3VA1180-6GD46-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 4-pole, line protection TM210, FTFM, In=80A overload protection Ir=80A fixed short-circuit protection Ii=10 x In N conductor protection 100% clamp connection",294,"ST",null,"LP",1.17,1,"3VA11806GD460AA0"]
["3VA1196-3GF42-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 4-pole, line protection TM240, ATAM, In=16A overload protection Ir=11A...16A short-circuit protection Ii=10...20 x In N conductor protection 100% nut keeper kit",170,"ST",null,"LP",1.224,1,"3VA11963GF420AA0"]
["3VA1196-4EF32-0HH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=16A overload protection Ir=11A...16A short-circuit protection Ii=10...20 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",352,"ST",null,"LP",1.08,1,"3VA11964EF320HH0"]
["3VA1196-5GE46-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM220, ATFM, In=16A overload protection Ir=11A...16A short-circuit protection Ii=20 x In N conductor protection 100% clamp connection",253,"ST",null,"LP",1.17,1,"3VA11965GE460AA0"]
["3VA1216-4EF32-0AH0","circuit breaker 3VA1 IEC frame 250 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In nut keeper kit 2 auxiliary switches HQ 1 trip alarm switch HQ",424,"ST",null,"LP",1.89,1,"3VA12164EF320AH0"]
["3VA1216-6EF42-0AA0","circuit breaker 3VA1 IEC frame 250 breaking capacity class H Icu=70kA @ 415V 4-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In N conductor unprotected nut keeper kit",542,"ST",null,"LP",2.0760000000000001,1,"3VA12166EF420AA0"]
["3VA1220-5EF42-0DH0","circuit breaker 3VA1 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM240, ATAM, In=200A overload protection Ir=140A...200A short-circuit protection Ii=5...10 x In N conductor unprotected nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",668,"ST",null,"LP",2.2000000000000002,1,"3VA12205EF420DH0"]
["3VA1220-5MH32-0DA0","circuit breaker 3VA1 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, starter protection TM120M, AM, In=200A without overload protection short-circuit protection Ii=6...14 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz",643,"ST",null,"LP",1.98,1,"3VA12205MH320DA0"]
["3VA1220-6EF32-0JA0","circuit breaker 3VA1 IEC frame 250 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=200A overload protection Ir=140A...200A short-circuit protection Ii=5...10 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz",471,"ST",null,"LP",1.89,1,"3VA12206EF320JA0"]
["3VA1225-4EF32-0AG0","circuit breaker 3VA1 IEC frame 250 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=250A overload protection Ir=175A...250A short-circuit protection Ii=5...10 x In nut keeper kit 1 auxiliary switch HP 1 trip alarm switch HP",418,"ST",null,"LP",1.873,1,"3VA12254EF320AG0"]
["3VA1225-4GF42-0HA0","circuit breaker 3VA1 IEC frame 250 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM240, ATAM, In=250A overload protection Ir=175A...250A short-circuit protection Ii=5...10 x In N conductor protection 100% nut keeper kit shunt trip (STL) 12-30V DC; 24V AC 50/60Hz",814,"ST",null,"LP",2.2000000000000002,1,"3VA12254GF420HA0"]
["3VA1225-5FF42-0CA0","circuit breaker 3VA1 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM240, ATAM, In=250A overload protection Ir=175A...250A short-circuit protection Ii=5...10 x In N conductor protection 50% nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz",902,"ST",null,"LP",2.39,1,"3VA12255FF420CA0"]
["3VA1225-6EF32-0CA0","circuit breaker 3VA1 IEC frame 250 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=250A overload protection Ir=175A...250A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz",455,"ST",null,"LP",1.89,1,"3VA12256EF320CA0"]
["3VA1340-7EF32-0AA0","circuit breaker 3VA1 IEC frame 400 breaking capacity class C Icu=110kA @ 415 V 3-pole, line protection TM240,  ATAM, In=400A overload protection Ir=280A ...400A short-circuit protection Ii=5...10 x In nut keeper kit",858,"ST",null,"LP",4.9279999999999999,1,"3VA13407EF320AA0"]
["3VA1463-5EF42-0AB0","circuit breaker 3VA1 IEC frame 630 breaking capacity class M Icu=55kA @ 415 V 4-pole, line protection TM240,  ATAM, In=630A overload protection ir=441a ...630A short circuit protection iI=5...10 x In neutral Unprotected busbar connection circuit breaker 3VA1 IEC frame 630 breaking capacity class M Icu=55kA @ 415 V 4-pole, line protection TM240, ATAM, In=630A overload protection ir=441a ...630A short circuit 2 auxiliary switch changeover H",1327,"ST",null,"LP",6.8780000000000001,1,"3VA14635EF420AB0"]
["3VA2010-5HL36-0HH0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=100A overload protection Ir=40A...100A short-circuit protection Ii=1.5...12 x In clamp connection shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",456,"ST",null,"LP",2.61,1,"3VA20105HL360HH0"]
["3VA2010-5JQ32-0AC0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU560, LSIG, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit 2 auxiliary switches HQ",747,"ST",null,"LP",2.35,1,"3VA20105JQ320AC0"]
["3VA2010-5KP32-0HA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU850, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer nut keeper kit shunt trip (STL) 12-30V DC; 24V AC 50/60Hz",742,"ST",null,"LP",2.39,1,"3VA20105KP320HA0"]
["3VA2010-6HN36-0DC0","circuit breaker 3VA2 IEC frame 100 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In clamp connection undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",533,"ST",null,"LP",2.61,1,"3VA20106HN360DC0"]
["3VA2025-5JQ36-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU560, LSIG, In=25A overload protection Ir=10A...25A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s clamp connection",712,"ST",null,"LP",2.5,1,"3VA20255JQ360AA0"]
["3VA2025-7JP42-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class C Icu=110kA @ 415V 4-pole, line protection ETU550, LSI, In=25A overload protection Ir=10A...25A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) nut keeper kit",687,"ST",null,"LP",3.2,1,"3VA20257JP420AA0"]
["3VA2040-6HN36-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=40A overload protection Ir=16A...40A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In clamp connection",401,"ST",null,"LP",2.2650000000000001,1,"3VA20406HN360AA0"]
["3VA2063-5HL32-0AJ0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=63A overload protection Ir=25A...63A short-circuit protection Ii=1.5...12 x In nut keeper kit 2 auxiliary switches HP 1 trip alarm switch HP",382,"ST",null,"LP",2.4,1,"3VA20635HL320AJ0"]
["3VA2063-5HL36-0AJ0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=63A overload protection Ir=25A...63A short-circuit protection Ii=1.5...12 x In clamp connection 2 auxiliary switches HP 1 trip alarm switch HP",399,"ST",null,"LP",2.5499999999999998,1,"3VA20635HL360AJ0"]
["3VA2063-5JQ32-0AC0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU560, LSIG, In=63A overload protection Ir=25A...63A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer gr.-fault prot., can be sw. off Ig=0.25...1 x In, tg=0.05-0.8s nut keeper kit 2 auxiliary switches HQ",732,"ST",null,"LP",2.35,1,"3VA20635JQ320AC0"]
["3VA2063-5KP32-0HA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU850, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer nut keeper kit shunt trip (STL) 12-30V DC; 24V AC 50/60Hz",727,"ST",null,"LP",2.39,1,"3VA20635KP320HA0"]
["3VA2063-6HN32-0AF0","circuit breaker 3VA2 IEC frame 100 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit 1 auxiliary switch HQ 1 trip alarm switch HQ",416,"ST",null,"LP",2.34,1,"3VA20636HN320AF0"]
["3VA2063-8HL46-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class L Icu=150kA @ 415V 4-pole, line protection ETU320, LI, In=63A overload protection Ir=25A...63A short-circuit protection Ii=1.5...12 x In N conductor protection adjustable (OFF, 100%) clamp connection",556,"ST",null,"LP",3.2,1,"3VA20638HL460AA0"]
["3VA2110-5HN32-0KH0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ",479,"ST",null,"LP",2.46,1,"3VA21105HN320KH0"]
["3VA2110-5HN36-0KH0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In clamp connection shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ",495,"ST",null,"LP",2.61,1,"3VA21105HN360KH0"]
["3VA2110-5MN32-0CH0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",477,"ST",null,"LP",2.4,1,"3VA21105MN320CH0"]
["3VA2110-5MN36-0KA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=3...15 x Ir, Ii=15 x In clamp connection shunt trip (STL) 220-250V DC, 208-277V AC",428,"ST",null,"LP",2.5,1,"3VA21105MN360KA0"]
["3VA2110-6HN36-0BL0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In clamp connection undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",574,"ST",null,"LP",2.67,1,"3VA21106HN360BL0"]
["3VA2110-7HN46-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 4-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In N conductor protection adjustable (OFF, 50%, 100%) clamp connection",574,"ST",null,"LP",3.2,1,"3VA21107HN460AA0"]
["3VA2110-7MS32-0HH0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 3-pole, starter protection ETU310M, I, In=100A overload protection Ir=40A...100A short-circuit protection Ii=3...15 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",403,"ST",null,"LP",2.4,1,"3VA21107MS320HH0"]
["3VA2110-7MS36-0HH0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 3-pole, starter protection ETU310M, I, In=100A overload protection Ir=40A...100A short-circuit protection Ii=3...15 x In clamp connection shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",417,"ST",null,"LP",2.5,1,"3VA21107MS360HH0"]
["3VA2116-5HL32-0BA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=160A overload protection Ir=63A...160A short-circuit protection Ii=1.5...10 x In nut keeper kit undervoltage release (UVR) 24V DC",580,"ST",null,"LP",2.4,1,"3VA21165HL320BA0"]
["3VA2116-5HN36-0CC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=160A overload protection Ir=63A...160A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In clamp connection undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ",665,"ST",null,"LP",2.61,1,"3VA21165HN360CC0"]
["3VA2116-5JQ32-0HH0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU560, LSIG, In=160A overload protection Ir=63A...160A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit shunt trip (STL) 12-30V DC; 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",959,"ST",null,"LP",2.4700000000000002,1,"3VA21165JQ320HH0"]
["3VA2116-6HN32-0CH0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=160A overload protection Ir=63A...160A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",727,"ST",null,"LP",2.4900000000000002,1,"3VA21166HN320CH0"]
["3VA2116-6KP46-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 4-pole, line protection ETU850, LSI, In=160A overload protection Ir=63A...160A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection adjustable (OFF, up to 100%) clamp connection",1075,"ST",null,"LP",3.2,1,"3VA21166KP460AA0"]
["3VA2125-6KQ42-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 4-pole, line protection ETU860, LSIG, In=25A overload protection Ir=10A...25A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) gr.-fault prot., can be sw. off Ig=0.2...1 x In= tg=0.05-0.8s nut keeper kit",868,"ST",null,"LP",3.2,1,"3VA21256KQ420AA0"]
["3VA2125-8HN42-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class L Icu=150kA @ 415V 4-pole, line protection ETU350, LSI, In=25A overload protection Ir=10A...25A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In N conductor protection adjustable (OFF, 100%) nut keeper kit",573,"ST",null,"LP",3.2,1,"3VA21258HN420AA0"]
["3VA2140-6JQ32-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU560, LSIG, In=40A overload protection Ir=16A...40A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.4... 1 x In, tg=0.05-0.8s nut keeper kit",737,"ST",null,"LP",2.5,1,"3VA21406JQ320AA0"]
["3VA2140-7JP42-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 4-pole, line protection ETU550, LSI, In=40A overload protection Ir=16A...40A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) nut keeper kit",687,"ST",null,"LP",3.2,1,"3VA21407JP420AA0"]
["3VA2163-5HL36-0DA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=63A overload protection Ir=25A...63A short-circuit protection Ii=1.5...12 x In clamp connection undervoltage release (UVR) 208-230V AC 50/60Hz",401,"ST",null,"LP",2.5499999999999998,1,"3VA21635HL360DA0"]
["3VA2163-5HN36-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In clamp connection",366,"ST",null,"LP",2.2909999999999999,1,"3VA21635HN360AA0"]
["3VA2163-5KP32-0CC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU850, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ",767,"ST",null,"LP",2.48,1,"3VA21635KP320CC0"]
["3VA2163-5KQ42-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU860, LSIG, In=63A overload protection Ir=25A...63A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) gr.-fault prot., can be sw. off Ig=0.25...1 x In= tg=0.05-0.8s nut keeper kit",828,"ST",null,"LP",3.2,1,"3VA21635KQ420AA0"]
["3VA2163-6HL36-0HL0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU320, LI, In=63A overload protection Ir=25A...63A short-circuit protection Ii=1.5...12 x In clamp connection shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",487,"ST",null,"LP",2.64,1,"3VA21636HL360HL0"]
["3VA2163-6HN32-0DC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",488,"ST",null,"LP",2.46,1,"3VA21636HN320DC0"]
["3VA2163-6JQ36-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU560, LSIG, In=63A overload protection Ir=25A...63A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.25...1 x In, tg=0.05-0.8s clamp connection",747,"ST",null,"LP",2.5,1,"3VA21636JQ360AA0"]
["3VA2163-7MN32-0JL0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 3-pole, motor protection ETU350M, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",524,"ST",null,"LP",2.2839999999999998,1,"3VA21637MN320JL0"]
["3VA2163-8HN42-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class L Icu=150kA @ 415V 4-pole, line protection ETU350, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In N conductor protection adjustable (OFF, 100%) nut keeper kit",573,"ST",null,"LP",3.2,1,"3VA21638HN420AA0"]
["3VA2216-5HM42-0AA0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU330, LIG, In=160A overload protection Ir=63A...160A short-circuit protection Ii=1.5...12 x In N conductor protection adjustable (OFF, 50%, 100%) ground-fault protection Ig=0.2...1 x In= tg=0.1/0.3s nut keeper kit",1033,"ST",null,"LP",2.8940000000000001,1,"3VA22165HM420AA0"]
["3VA2216-5MN32-0DH0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=160A overload protection Ir=63A...160A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",710,"ST",null,"LP",2.2839999999999998,1,"3VA22165MN320DH0"]
["3VA2220-5MN32-0DB0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=200A overload protection Ir=80A...200A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HP",800,"ST",null,"LP",2.3140000000000001,1,"3VA22205MN320DB0"]
["3VA2220-7MN32-0CA0","circuit breaker 3VA2 IEC frame 250 breaking capacity class C Icu=110kA @ 415V 3-pole, motor protection ETU350M, LSI, In=200A overload protection Ir=80A...200A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz",880,"ST",null,"LP",2.4,1,"3VA22207MN320CA0"]
["3VA2225-5HN32-0AC0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In nut keeper kit 2 auxiliary switches HQ",732,"ST",null,"LP",2.4500000000000002,1,"3VA22255HN320AC0"]
["3VA2225-5HN42-0AA0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU350, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In N conductor protection adjustable (OFF, 50%, 100%) nut keeper kit",902,"ST",null,"LP",2.8580000000000001,1,"3VA22255HN420AA0"]
["3VA2225-5KP32-0AD0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU850, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer nut keeper kit 3 auxiliary switches HQ",1029,"ST",null,"LP",2.5099999999999998,1,"3VA22255KP320AD0"]
["3VA2225-5KP42-0AE0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU850, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection adjustable (OFF, up to 100%) nut keeper kit circuit breaker 3VA2 IEC frame 250 4 auxiliary switches HQ",1205,"ST",null,"LP",3.0339999999999998,1,"3VA22255KP420AE0"]
["3VA2225-6JQ32-0CH0","circuit breaker 3VA2 IEC frame 250 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU560, LSIG, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",1191,"ST",null,"LP",2.61,1,"3VA22256JQ320CH0"]
["3VA2225-6KP32-0DH0","circuit breaker 3VA2 IEC frame 250 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU850, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",1171,"ST",null,"LP",2.5299999999999998,1,"3VA22256KP320DH0"]
["3VA2225-7HL32-0KL0","circuit breaker 3VA2 IEC frame 250 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU320, LI, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...10 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",931,"ST",null,"LP",2.6,1,"3VA22257HL320KL0"]
["3VA2225-8HL32-0JH0","circuit breaker 3VA2 IEC frame 250 breaking capacity class L Icu=150kA @ 415V 3-pole, line protection ETU320, LI, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...10 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",1033,"ST",null,"LP",2.57,1,"3VA22258HL320JH0"]
["3VA2325-5MN32-0AE0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit 4 auxiliary switches HQ",1027,"ST",null,"LP",4.3,1,"3VA23255MN320AE0"]
["3VA2325-6HL32-0DC0","circuit breaker 3VA2 IEC frame 400 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU320, LI, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...12 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",1090,"ST",null,"LP",4.3,1,"3VA23256HL320DC0"]
["3VA2325-7MN32-0DC0","circuit breaker 3VA2 IEC frame 400 breaking capacity class C Icu=110kA @ 415V 3-pole, motor protection ETU350M, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",1220,"ST",null,"LP",4.3,1,"3VA23257MN320DC0"]
["3VA2340-5HL32-0DL0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=400A overload protection Ir=160A...400A short-circuit protection Ii=1.5...10 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",1016,"ST",null,"LP",4.3,1,"3VA23405HL320DL0"]
["3VA2340-5HN32-0AF0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In nut keeper kit 1 auxiliary switch HQ 1 trip alarm switch HQ",971,"ST",null,"LP",4.4000000000000004,1,"3VA23405HN320AF0"]
["3VA2340-5JQ32-0BA0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU560, LSIG, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6...10 x In, Ii=1.5 x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit undervoltage release (UVR) 24V DC",1281,"ST",null,"LP",4.4000000000000004,1,"3VA23405JQ320BA0"]
["3VA2340-5JQ42-0KH0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU560, LSIG, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6...10 x In, Ii=1.5 x In N conductor protection adjustable (OFF, up to 100%) gr.-fault prot., can be sw. off Ig=0.2...1 x In= tg=0.05-0.8s nut keeper kit shunt trip (STL) 220-250V DC; 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ",1558,"ST",null,"LP",5.8,1,"3VA23405JQ420KH0"]
["3VA2340-6HN32-0AD0","circuit breaker 3VA2 IEC frame 400 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In nut keeper kit 3 auxiliary switches HQ",1090,"ST",null,"LP",4.4000000000000004,1,"3VA23406HN320AD0"]
["3VA2340-6JP32-0KH0","circuit breaker 3VA2 IEC frame 400 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU550, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6...10 x In, Ii=1.5 x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit shunt trip (STL) 220-250V DC; 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ",1266,"ST",null,"LP",4.4000000000000004,1,"3VA23406JP320KH0"]
["3VA2340-7HN32-0HA0","circuit breaker 3VA2 IEC frame 400 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU350, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz",1186,"ST",null,"LP",4.4000000000000004,1,"3VA23407HN320HA0"]
["3VA2440-5HL32-0BC0","circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=400A overload protection Ir=160A...400A short-circuit protection Ii=1.5...12 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ",1283,"ST",null,"LP",4.3,1,"3VA24405HL320BC0"]
["3VA2440-6HL32-0JA0","circuit breaker 3VA2 IEC frame 630 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU320, LI, In=400A overload protection Ir=160A...400A short-circuit protection Ii=1.5...12 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz",1396,"ST",null,"LP",4.3,1,"3VA24406HL320JA0"]
["3VA2440-6HN32-0HA0","circuit breaker 3VA2 IEC frame 630 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz",1452,"ST",null,"LP",4.4000000000000004,1,"3VA24406HN320HA0"]
["3VA2450-5MN32-0CC0","circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=500A overload protection Ir=200A...500A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz",1611,"ST",null,"LP",4.4000000000000004,1,"3VA24505MN320CC0"]
["3VA2450-7MN32-0BH0","circuit breaker 3VA2 IEC frame 630 breaking capacity class C Icu=110kA @ 415V 3-pole, motor protection ETU350M, LSI, In=500A overload protection Ir=200A...500A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ",1917,"ST",null,"LP",4.4000000000000004,1,"3VA24507MN320BH0"]
["3VA2463-5HN42-0KH0","circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU350, LSI, In=630A overload protection Ir=250A...630A short-circuit protection Isd=1.5...9x Ir, Ii=9x In N conductor protection adjustable (OFF, 50%, 100%) nut keeper kit shunt trip (STL) 220-250V DC; 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ",1731,"ST",null,"LP",6.867,1,"3VA24635HN420KH0"]
["3VA2463-5JP32-0KL0","circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU550, LSI, In=630A overload protection Ir=250A...630A short-circuit protection Isd=0.6..9 x In, Ii=1.5..9 x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit shunt trip (STL) 220-250V DC; 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",1453,"ST",null,"LP",4.4000000000000004,1,"3VA24635JP320KL0"]
["3VA2463-5KP32-0DH0","circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU850, LSI, In=630A overload protection Ir=250A...630A short-circuit protection Isd=0.6..9 x In, Ii=1.5..9 x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",1574,"ST",null,"LP",4.4000000000000004,1,"3VA24635KP320DH0"]
["3VA2463-6HN42-0AA0","circuit breaker 3VA2 IEC frame 630 breaking capacity class H Icu=85kA @ 415V 4-pole, line protection ETU350, LSI, In=630A overload protection Ir=250A...630A short-circuit protection Isd=1.5...9x Ir, Ii=9x In N conductor protection adjustable (OFF, 50%, 100%) nut keeper kit",1844,"ST",null,"LP",6.726,1,"3VA24636HN420AA0"]
["3VA2463-6KP32-0AC0","circuit breaker 3VA2 IEC frame 630 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU850, LSI, In=630A overload protection Ir=250A...630A short-circuit protection Isd=0.6..9 x In, Ii=1.5..9 x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit 2 auxiliary switches HQ",1639,"ST",null,"LP",4.4000000000000004,1,"3VA24636KP320AC0"]
["3VA2463-7HN42-0DD0","circuit breaker 3VA2 IEC frame 630 breaking capacity class C Icu=110kA @ 415V 4-pole, line protection ETU350, LSI, In=630A overload protection Ir=250A...630A short-circuit protection Isd=1.5...9x Ir, Ii=9x In N conductor protection adjustable (OFF, 50%, 100%) nut keeper kit circuit breaker 3VA2 IEC frame 630 undervoltage release 208-230V AC 50/60Hz 3 auxiliary switches HQ",1853,"ST",null,"LP",5.1529999999999996,1,"3VA24637HN420DD0"]
["3VA2510-5KQ32-0HL0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU860, LSIG, In=1000A overload protection Ir=400A...1000A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection, opt. w. ext. curr. transf., up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In= tg=0.05-0.8s nut keeper kit shunt trip (STL) 12-30V DC; 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",2702,"ST",null,"LP",14.2,1,"3VA25105KQ320HL0"]
["3VA2510-6JP42-0AA0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class H Icu=85kA @ 415V 4-pole, line protection ETU550, LSI, In=1000A overload protection Ir=400A...1000A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection adjustable (OFF, up to 100%) nut keeper kit",3383,"ST",null,"LP",16.78,1,"3VA25106JP420AA0"]
["3VA2580-5HL32-0HC0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=800A overload protection Ir=320A...800A short-circuit protection Ii=1.5...12 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ",1748,"ST",null,"LP",14.2,1,"3VA25805HL320HC0"]
["3VA2580-5JP32-0DH0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU550, LSI, In=800A overload protection Ir=320A...800A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",1846,"ST",null,"LP",14.2,1,"3VA25805JP320DH0"]
["3VA2580-6HM32-0AA0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU330, LIG, In=800A overload protection Ir=320A...800A short-circuit protection Ii=1.5...12 x In ground-fault protection Ig=0.2...1 x In, tg=0.1/0.3s nut keeper kit",2042,"ST",null,"LP",11.34,1,"3VA25806HM320AA0"]
["3VA5112-5ED31-1AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class M 35kA @ 480V 3-pole, line protection TM210, FTFM, In=125A overload protection Ir=125A fixed short-circuit protection Ii=10 x In UL 489 SB (naval), 50Β° C without connection",420,"ST",null,"LP",0.88,1,"3VA51125ED311AA0"]
["3VA5130-5ED11-0AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class M 35kA @ 277V 1-pole, line protection TM210, FTFM, In=30A overload protection Ir=30A fixed short-circuit protection Ii=10 x In without connection",97.8,"ST",null,"LP",0.38300000000000001,1,"3VA51305ED110AA0"]
["3VA5145-5ED31-1AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class M 35kA @ 480 V 3-pole, line protection TM210, FTFM, In=45A overload protection Ir=45A fixed short-circuit protection Ii=10 x In UL 489 SB (naval), 50Β° C without connection",201,"ST",null,"LP",0.88,1,"3VA51455ED311AA0"]
["3VA5190-1MU31-0AA0","circuit breaker 3VA5 UL frame 125 3-pole, starter protection TM120M, AM, In=90A without overload protection short-circuit protection Ii=3...7 x In without connection",251,"ST",null,"LP",0.96299999999999997,1,"3VA51901MU310AA0"]
["3VA5217-6EC61-0AA0","circuit breaker 3VA5 UL frame 250 breaking capacity class H 65kA @ 480V 2-pole, line protection TM230, FTAM, In=175A overload protection Ir=175A fixed short-circuit protection Ii=5...10 x In without connection",637,"ST",null,"LP",1.84,1,"3VA52176EC610AA0"]
["3VA5222-5EC31-0AA0","circuit breaker 3VA5 UL frame 250 breaking capacity class M 35kA @ 480V 3-pole, line protection TM230, FTAM, In=225A overload protection Ir=225A fixed short-circuit protection Ii=5...10 x In without connection",706,"ST",null,"LP",2.0459999999999998,1,"3VA52225EC310AA0"]
["3VA6110-5HN41-0AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class M 35kA @ 480V 4-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In N conductor protection adjustable (OFF, 50%, 100%) without connection",596,"ST",null,"LP",3.2,1,"3VA61105HN410AA0"]
["3VA6110-7KP31-0AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class C 100kA @ 480V 3-pole, line protection ETU850, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% without connection",1122,"ST",null,"LP",2.5,1,"3VA61107KP310AA0"]
["3VA6115-5KP31-2AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class M 35kA @ 480V 3-pole, line protection ETU850, LSI, In=150A overload protection Ir=60A...150A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer, up to 160% without connection",1368,"ST",null,"LP",2.2999999999999998,1,"3VA61155KP312AA0"]
["3VA6115-7JT31-0AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class C 100kA @ 480V 3-pole, line protection ETU556, LSI, In=150A overload protection Ir=60A...150A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer, up to 160% ground-fault alarm message via EFB300 or COM without connection",1204,"ST",null,"LP",2.5,1,"3VA61157JT310AA0"]
["3VA6115-8HN31-2AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class L 150kA @ 480V 3-pole, line protection ETU350, LSI, In=150A overload protection Ir=60A...150A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In without connection",1053,"ST",null,"LP",2.2999999999999998,1,"3VA61158HN312AA0"]
["3VA6140-6KM31-2AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class H 65kA @ 480V 3-pole, line protection ETU830, LIG, In=40A overload protection Ir=16A...40A short-circuit protection Ii=1.5...12 x In ground-fault protection Ig=0.375...1 x In, tg=0.05-0.8s without connection",1286,"ST",null,"LP",2.2999999999999998,1,"3VA61406KM312AA0"]
["3VA6140-7KT31-0AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class C 100kA @ 480V 3-pole, line protection ETU856, LSI, In=40A overload protection Ir=16A...40A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% ground-fault alarm message via EFB300 or COM without connection",1072,"ST",null,"LP",2.5,1,"3VA61407KT310AA0"]
["3VA6210-5JT31-0AA0","circuit breaker 3VA6 UL frame 250 breaking capacity class M 35kA @ 480V 3-pole, line protection ETU556, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% ground-fault alarm message via EFB300 or COM without connection",1267,"ST",null,"LP",2.5,1,"3VA62105JT310AA0"]
["3VA6210-7KL31-2AA0","circuit breaker 3VA6 UL frame 250 breaking capacity class C 100kA @ 480V 3-pole, line protection ETU820, LI, In=100A overload protection Ir=40A...100A short-circuit protection Ii=1.5...12 x In without connection",1759,"ST",null,"LP",2.2999999999999998,1,"3VA62107KL312AA0"]
["3VA6225-5KT41-0AA0","circuit breaker 3VA6 UL frame 250 breaking capacity class M 35kA @ 480V 4-pole, line protection ETU856, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection adjustable (OFF, up to 100%) ground-fault alarm message via EFB300 or COM without connection",1727,"ST",null,"LP",3.2,1,"3VA62255KT410AA0"]
["3VA6225-6KM31-2AA0","circuit breaker 3VA6 UL frame 250 breaking capacity class H 65kA @ 480V 3-pole, line protection ETU830, LIG, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...10 x In ground-fault protection Ig=0.2...1 x In, tg=0.05-0.8s without connection",1866,"ST",null,"LP",2.2999999999999998,1,"3VA62256KM312AA0"]
["3VA6325-5KL41-2AA0","circuit breaker 3VA6 UL frame 400 breaking capacity class M 35kA @ 480V 4-pole, line protection ETU820, LI, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...12 x In without connection",2219,"ST",null,"LP",6.9,1,"3VA63255KL412AA0"]
["3VA6325-6KQ41-0AA0","circuit breaker 3VA6 UL frame 400 breaking capacity class H 65kA @ 480V 4-pole, line protection ETU860, LSIG, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) ground-fault protection Ig=0.2...1 x In= tg=0.05-0.8s without connection",2363,"ST",null,"LP",6.9,1,"3VA63256KQ410AA0"]
["3VA6340-5KP41-0AA0","circuit breaker 3VA6 UL frame 400 breaking capacity class M 35kA @ 480V 4-pole, line protection ETU850, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection adjustable (OFF, up to 100%) without connection",2092,"ST",null,"LP",6.9,1,"3VA63405KP410AA0"]
["3VA6340-7HN31-0AA0","circuit breaker 3VA6 UL frame 400 breaking capacity class C 100kA @ 480V 3-pole, line protection ETU350, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In without connection",1463,"ST",null,"LP",5.3,1,"3VA63407HN310AA0"]
["3VA6440-6JT41-2AA0","circuit breaker 3VA6 UL frame 600 breaking capacity class H 65kA @ 480V 4-pole, line protection ETU556, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) ground-fault alarm message via EFB300 or COM without connection",3290,"ST",null,"LP",6.9,1,"3VA64406JT412AA0"]
["3VA6440-7KP41-0AA0","circuit breaker 3VA6 UL frame 600 breaking capacity class C 100kA @ 480V 4-pole, line protection ETU850, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) without connection",3145,"ST",null,"LP",6.9,1,"3VA64407KP410AA0"]
["3VA6460-7JT41-0AA0","circuit breaker 3VA6 UL frame 600 breaking capacity class C 100kA @ 480V 4-pole, line protection ETU556, LSI, In=600A overload protection Ir=240A...600A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection adjustable (OFF, up to 100%) ground-fault alarm message via EFB300 or COM without connection",2949,"ST",null,"LP",6.9,1,"3VA64607JT410AA0"]
["3VA6460-8KQ31-0AA0","circuit breaker 3VA6 UL frame 600 breaking capacity class L 150kA @ 480V 3-pole, line protection ETU860, LSIG, In=600A overload protection Ir=240A...600A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer, up to 160% ground-fault protection Ig=0.2...1 x In, tg=0.05-0.8s without connection",2936,"ST",null,"LP",5.3,1,"3VA64608KQ310AA0"]
["3VA9113-0JF60","distribution wire connector 6 cables 3 units accessory for: 3VA1 100/160",68.8,"ST",null,"LP",0.34399999999999997,1,"3VA91130JF60"]
["3VA9138-0CK12","operating unit w. Bowden cable Max Flex operator complete kit comprising: handle steel, epoxy sheathed NEMA 1/3R/12; Bowden cable length 0.9m (36\"); switching mechanism accessory for: 3VA5 125",441,"ST",null,"LP",2.4609999999999999,1,"3VA91380CK12"]
["3VA9154-0QC00","bus connector offset front 4 units accessory for: 3VA1 100/160",49.6,"ST",null,"LP",0.20200000000000001,1,"3VA91540QC00"]
["3VA9214-0KP00","plug-in unit complete kit accessory for: circuit breaker, 4-pole 3VA1 250",207,"ST",null,"LP",2.17,1,"3VA92140KP00"]
["3VA9243-0JJ13","wire connector large 3 units accessory for: 3VA6 150/250",56.9,"ST",null,"LP",0.503,1,"3VA92430JJ13"]
["3VA9264-0QB00","bus connector extended front 4 units accessory for: 3VA2 100/160/250",30.2,"ST",null,"LP",0.34200000000000003,1,"3VA92640QB00"]
["3VA9271-0WD40","terminal cover 4-pole 1 unit accessory for: 3VA6 150/250 3VA5 250 plug-in/draw-out socket 3VA6 150/250",19.100000000000001,"ST",null,"LP",3.7999999999999999E-2,1,"3VA92710WD40"]
["3VA9373-0JF60","distribution wire connector 6 cables 3 units accessory for: plug-in/draw-out unit 3VA6 400/600",82.7,"ST",null,"LP",0.66200000000000003,1,"3VA93730JF60"]
["3VA9447-0EK17","FRONT MOUNTED ROTARY OPERATOR EMERGENCY-OFF IEC IP30/40 ILLUMINATION KIT 24 V DC ACCESSORY FOR: 3VA5/6 400/600",112,"ST",null,"LP",0.371,1,"3VA94470EK17"]
["3VA9504-0JB23","WIRE CONNECTOR 2 CABLES 4 PCS. ACCESSORY FOR: 3VA15/25 1000",138,"ST",null,"LP",1.4890000000000001,1,"3VA95040JB23"]
["3VA9908-0BB20","UNDERVOLTAGE RELEASE 24 V AC 50/60HZ ACCESSORY FOR 3VA1 and 3VA20 up to 3VA25",73.8,"ST",null,"LP",8.5999999999999993E-2,1,"3VA99080BB20"]
["3VA9988-0AB12","TRIP ALARM SWITCH CHANGEOVER CONTACTS TYPE HQ (7MM) ACCESSORY FOR 3VA1 and 3VA20 up to 3VA25",15.3,"ST",null,"LP",2.7E-2,1,"3VA99880AB12"]
["3VL1105-1KM30-0AA0","circuit breaker VL150X UL, type CG (cat no. NCX3B050) non-interchangeable frame, with circuit breaker approval acc. to UL 489 standard breaking capacity 3-pole, NEMA rating 35kA/480V (molded case circuit breaker) Electronic Trip Unit TM, LI function TA=40Β°C In=<50A rated current II=600A short-circuit protection Ir=50A Electronic Trip Unit for line protection without connection accessories without auxiliary release without auxiliary/alarm switch",319,"ST",null,"LP",2,1,"3VL11051KM300AA0"]
["3VL1705-2DD33-0AA0","circuit breaker VL160X H high breaking capacity Icu=70kA, 415V AC 3-pole, line protection Electronic Trip Unit TM, LI In=50A, rated current Ir=50A, overload protection II=600A, short-circuit prot. without auxiliary release without auxiliary/alarm switch",297,"ST",null,"LP",2.21,1,"3VL17052DD330AA0"]
["3VL1706-1EA46-0AA0","circuit breaker VL160X N standard breaking capacity Icu=55kA, 415V AC 4-pole, line protection Electronic Trip Unit TM, LI In=63A, rated current Ir=63A, overload protection II=600A, short-circuit prot. N protected with screw terminals without auxiliary release without auxiliary/alarm switch",310,"ST",null,"LP",2.698,1,"3VL17061EA460AA0"]
["3VL1710-1DA36-2JA0","circuit breaker VL160X N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection Electronic Trip Unit TM, LI In=100A, rated current Ir=100A, overload protection II=1000A, short-circuit prot. with screw terminals Undervoltage release 380...415 V AC without auxiliary/alarm switch","On Request","ST",null,"LP",2,1,"3VL17101DA362JA0"]
["3VL1716-1DE36-0AB1","circuit breaker VL160X N standard breaking capacity Icu=55kA, 415V AC 3-pole, non-auto. air circ. br. Electronic Trip Unit magnetic In=160A, rated current II=1800A, short-circuit prot. with screw terminals without auxiliary release Auxiliary switch mounting kit 2 AUX (1 NO + 1 NC)","On Request","ST",null,"LP",2,1,"3VL17161DE360AB1"]
["3VL2508-3KN30-0AA0","circuit breaker VL150 UL type DG (cat no. LDK3B080) non-interchangeable frame, with circuit breaker approval acc. to UL 489 very high breaking capacity 3-pole; NEMA rating 100KA@480V and 18KA@600/347V (molded case circuit breaker) Electronic Trip Unit TM, LI TA=40Β°C In=80A, rated current II=450...800A short-circuit protection Ir=80A Electronic Trip Unit for line protection without connection accessories without auxiliary release without auxiliary/alarm switch",634,"ST",null,"LP",2.2000000000000002,1,"3VL25083KN300AA0"]
["3VL2515-3PD30-0AA0","circuit breaker VL150 UL type DG (cat no. LDK3W150) non-interchangeable frame, with circuit breaker approval acc. to UL 489 very high breaking capacity 3-pole; NEMA rating 100KA@480V and 18KA@600/347V (molded case circuit breaker) Electronic Trip Unit ETU, LIG TA=40Β°C 3 phases/4 lines In=150A, rated current II=1.25-11 xIN, short-circuit protection Ir=60-150A Electronic Trip Unit for line protection without connection accessories without auxiliary/alarm switch",1239,"ST",null,"LP",2.4,1,"3VL25153PD300AA0"]
["3VL2706-1MP36-0AA0","circuit breaker VL160N standard breaking capacity Icu=55kA, 415V AC 3-pole, motor/generator prot. Electronic Trip Unit ETU10M, LI In=63A, rated current IR=25...63A, overload protection, II=1.25 to 11xIN, short-circuit protection with screw terminals without auxiliary release ETU communication-capable without auxiliary/alarm switch",536,"ST",null,"LP",2.4470000000000001,1,"3VL27061MP360AA0"]
["3VL2706-1TH43-0AA0","circuit breaker VL160N standard breaking capacity Icu=55kA, 415V AC 4-pole, line protection Electronic Trip Unit ETU22, LSIG In=63A, rated current IR=25...63A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection N protected without auxiliary release without auxiliary/alarm switch",949,"ST",null,"LP",3.1349999999999998,1,"3VL27061TH430AA0"]
["3VL2706-2MS33-0AA0","circuit breaker VL160H high breaking capacity Icu=70kA, 415V AC 3-pole, motor protection Electronic Trip Unit ETU30M, LI Ir=25...63A, overload prot., TC=10A...30, II=6/8/11 xIN, short-circuit protection without auxiliary release ETU communication-capable without auxiliary/alarm switch",702,"ST",null,"LP",2.4470000000000001,1,"3VL27062MS330AA0"]
["3VL2706-3SG33-0AA0","circuit breaker VL160L very high breaking capacity Icu=100kA, 415V AC 3-pole, line protection Electronic Trip Unit ETU22, LSIG 3 phases/3 lines In=63A, rated current IR=26...63A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection without auxiliary release without auxiliary/alarm switch",968,"ST",null,"LP",2.4,1,"3VL27063SG330AA0"]
["3VL2708-1EM43-0AB1","circuit breaker VL160N standard breaking capacity Icu=55kA, 415V AC 4-pole, line protection Electronic Trip Unit TM, LI In=80A, rated current IR=63...80A, overload protection, II=400...800A, short-circuit protection N protected without auxiliary release Auxiliary switch mounting kit 2 AUX (1 NO + 1 NC)","On Request","ST",null,"LP",3,1,"3VL27081EM430AB1"]
["3VL2710-1SE36-0AB1","circuit breaker VL160N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection Electronic Trip Unit ETU20, LSI In=100A, rated current IR=40...100A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection with screw terminals without auxiliary release Auxiliary switch mounting kit 2 AUX (1 NO + 1 NC)","On Request","ST",null,"LP",2.4,1,"3VL27101SE360AB1"]
["3VL2710-1UN46-0AA0","circuit breaker VL160N standard breaking capacity Icu=55kA, 415V AC 4-pole, line protection Electronic Trip Unit LCD ETU42, LSIG In=100A, rated current IR=40...100A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection N protected with screw terminals without auxiliary release without auxiliary/alarm switch",1355,"ST",null,"LP",3.1,1,"3VL27101UN460AA0"]
["3VL2710-3DK36-0AA0","circuit breaker VL160L very high breaking capacity Icu=100kA, 415V AC 3-pole, starter combination Electronic Trip Unit magnetic In=100A, rated current II=750...1500A, short-circuit protection with screw terminals without auxiliary release without auxiliary/alarm switch",596,"ST",null,"LP",2.2000000000000002,1,"3VL27103DK360AA0"]
["3VL2710-3NA43-0AA0","circuit breaker VL160L very high breaking capacity Icu=100kA, 415V AC 4-pole, line protection Electronic Trip Unit ETU10, LIN In=100A, rated current IR=40...100A, overload protection, II=1.25 to 11xIN, short-circuit protection N protected without auxiliary release ETU communication-capable without auxiliary/alarm switch",1168,"ST",null,"LP",3.0779999999999998,1,"3VL27103NA430AA0"]
["3VL2712-1DC33-0AB1","circuit breaker VL160N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection Electronic Trip Unit TM, LI In=125A, rated current IR=100...125A, overload protection, II=625...1250A, short-circuit protection without auxiliary release Auxiliary switch mounting kit 2 AUX (1 NO + 1 NC)",706,"ST",null,"LP",2.4710000000000001,1,"3VL27121DC330AB1"]
["3VL2716-1LS36-0AA0","circuit breaker VL160N standard breaking capacity Icu=55kA, 415V AC 3-pole, motor protection Electronic Trip Unit ETU30M, LI IR=63...160A, overload prot., TC=10A...30, II=6/8/11 xIN, short-circuit protection with screw terminals without auxiliary release shipbuilding certificate for LRS, DNV and gL without auxiliary/alarm switch",1057,"ST",null,"LP",2.4470000000000001,1,"3VL27161LS360AA0"]
["3VL2716-2DC33-0AD1","circuit breaker VL160H high breaking capacity Icu=70kA, 415V AC 3-pole, line protection Electronic Trip Unit TM, LI In=160A, rated current IR=125...160A, overload protection, II=800...1600A, short-circuit protection without auxiliary release Auxiliary/alarm switch mounting kit 2 AUX (1 NO+1 NC)+1 AS (1 NO)",866,"ST",null,"LP",2.4609999999999999,1,"3VL27162DC330AD1"]
["3VL2716-2NE43-0AA0","circuit breaker VL160H high breaking capacity Icu=70kA, 415V AC 4-pole, line protection Electronic Trip Unit ETU20, LSI In=160A, rated current IR=64...160A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection without auxiliary release ETU communication-capable without auxiliary/alarm switch",1044,"ST",null,"LP",2.4470000000000001,1,"3VL27162NE430AA0"]
["3VL2716-3NH43-0AA0","circuit breaker VL160L very high breaking capacity Icu=100kA, 415V AC 4-pole, line protection Electronic Trip Unit ETU22, LSIG In=160A, rated current IR=64...160A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection N protected without auxiliary release ETU communication-capable without auxiliary/alarm switch",1549,"ST",null,"LP",2.4470000000000001,1,"3VL27163NH430AA0"]
["3VL2716-3UH33-0AA0","circuit breaker VL160L very high breaking capacity Icu=100kA, 415V AC 3-pole, line protection Electronic Trip Unit LCD ETU40, LI/LS/LSI In=160A, rated current IR=64...160A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection without auxiliary release without auxiliary/alarm switch",1247,"ST",null,"LP",2.4,1,"3VL27163UH330AA0"]
["3VL3115-2PH30-0AA0","circuit breaker VL250 UL; type FG (cat no. HFX3V150) non-interchangeable frame, with circuit breaker approval acc. to UL 489 high breaking capacity 3-pole, NEMA rating 65kA/480V, (molded case circuit breaker) Electronic Trip Unit ETU, LSIG TA=40Β°C 3 phases/4 lines In=150A, rated current ISD=1.5 to 10xIR, II=11X in short-circuit protection IR=60-150A Electronic Trip Unit for line protection without connection accessories without auxiliary release without auxiliary/alarm switch",1822,"ST",null,"LP",2.5,1,"3VL31152PH300AA0"]
["3VL3515-1PB30-0AA0","circuit breaker VL250 UL type FG (cat no. NFK3R150) non-interchangeable frame, with circuit breaker approval acc. to UL 489 standard breaking capacity 3-pole; NEMA rating 35KA@480V and 18KA@600/347V (molded case circuit breaker) Electronic Trip Unit ETU, LI TA=40Β°C In=150A, rated current II=1.25-11 xIN, short-circuit protection IR=60-150A Electronic Trip Unit for line protection without connection accessories without auxiliary/alarm switch",1194,"ST",null,"LP",2.5,1,"3VL35151PB300AA0"]
["3VL3720-1DC36-2JA0","circuit breaker VL250N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection Electronic Trip Unit TM, LI In=200A, rated current IR=160...200A, overload protection, II=1000...2000A, short-circuit protection Undervoltage release 380...415 V AC without auxiliary/alarm switch",775,"ST",null,"LP",2.64,1,"3VL37201DC362JA0"]
["3VL3720-2DC33-0AA0","circuit breaker VL250H high breaking capacity Icu=70kA, 415V AC 3-pole, line protection Electronic Trip Unit TM, LI In=200A, rated current IR=160...200A, overload protection, II=1000...2000A, short-circuit protection with box terminal without auxiliary release without auxiliary/alarm switch",797,"ST",null,"LP",2.2999999999999998,1,"3VL37202DC330AA0"]
["3VL3720-2MH36-0AA0","circuit breaker VL250H high breaking capacity Icu=70kA, 415V AC 3-pole, line protection Electronic Trip Unit ETU22, LSIG 3 phases/4 lines with connecting cable In=200A, rated current IR=80...200A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection without auxiliary release ETU communication-capable without auxiliary/alarm switch",1325,"ST",null,"LP",2.569,1,"3VL37202MH360AA0"]
["3VL3720-3TA46-0AA0","circuit breaker VL250L very high breaking capacity Icu=100kA, 415V AC 4-pole, line protection Electronic Trip Unit ETU10, LIN In=200A, rated current IR=80...200A, overload protection, II=1.25 to 11xIN, short-circuit protection N protected without auxiliary release without auxiliary/alarm switch",1612,"ST",null,"LP",3.3610000000000002,1,"3VL37203TA460AA0"]
["3VL3725-1DC33-2PD1","circuit breaker VL250N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection Electronic Trip Unit TM, LI In=250A, rated current IR=200...250A, overload protection, II=1200...2500A, short-circuit protection with box terminal Undervoltage release 24 V DC Auxiliary/alarm switch mounting kit 2 AUX (1 NO+1 NC)+1 AS (1 NO)","On Request","ST",null,"LP",2.2999999999999998,1,"3VL37251DC332PD1"]
["3VL3725-1SP33-0AA0","circuit breaker VL250N standard breaking capacity Icu=55kA, 415V AC 3-pole, motor/generator prot. Electronic Trip Unit ETU10M, LI In=250A, rated current IR=100...250A, overload protection, II=1.25 to 11xIN, short-circuit protection without auxiliary release with box terminal without auxiliary/alarm switch",840,"ST",null,"LP",2.7250000000000001,1,"3VL37251SP330AA0"]
["3VL3725-2DC36-0AA0","circuit breaker VL250H high breaking capacity Icu=70kA, 415V AC 3-pole, line protection Electronic Trip Unit TM, LI In=250A, rated current IR=200...250A, overload protection, II=1200...2500A, short-circuit protection without auxiliary release without auxiliary/alarm switch",819,"ST",null,"LP",2.581,1,"3VL37252DC360AA0"]
["3VL3725-2UL36-0AA0","circuit breaker VL250H high breaking capacity Icu=70kA, 415V AC 3-pole, line protection Electronic Trip Unit LCD ETU42, LSIG 3 phases/3 lines In=250A, rated current IR=100...250A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection without auxiliary release without auxiliary/alarm switch",1627,"ST",null,"LP",2.5750000000000002,1,"3VL37252UL360AA0"]
["3VL3725-3NB46-0AA0","circuit breaker VL250L very high breaking capacity Icu=100kA, 415V AC 4-pole, line protection Electronic Trip Unit ETU10, LI In=250A, rated current IR=100...250A, overload protection, II=1.25 to 11xIN, short-circuit protection without auxiliary release ETU communication-capable without auxiliary/alarm switch",1589,"ST",null,"LP",3.4529999999999998,1,"3VL37253NB460AA0"]
["3VL4140-3VH30-0AA0","circuit breaker VL400 UL type JG (cat no. LJX3A400) non-interchangeable frame, with circuit breaker approval acc. to UL 489 very high breaking capacity 3-pole; NEMA rating 100kA/480V and 25kA/600V (molded case circuit breaker) Electronic Trip Unit LCD ETU, LI/LS/LSI TA=40Β°C In=400A, rated current ISD=1.25-10xIR, II=11X in short-circuit protection IR=150-400A ETU for line protection without auxiliary release without auxiliary/alarm switch",3742,"ST",null,"LP",5.9,1,"3VL41403VH300AA0"]
["3VL4725-1DC36-2HA0","circuit breaker VL400N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection Electronic Trip Unit TM, LI In=250A, rated current IR=200...250A, overload protection, II=1200...2500A, short-circuit protection Undervoltage release 220...250 V AC without auxiliary/alarm switch","On Request","ST",null,"LP",5.7,1,"3VL47251DC362HA0"]
["3VL4731-1NN46-0AA0","circuit breaker VL400N standard breaking capacity Icu=55kA, 415V AC 4-pole, line protection Electronic Trip Unit ETU12, LIG In=315A, rated current IR=128...315A, overload protection, II=1.25 to 11xIN, short-circuit protection N protected without auxiliary release ETU communication-capable without auxiliary/alarm switch",2563,"ST",null,"LP",7.9409999999999998,1,"3VL47311NN460AA0"]
["3VL4731-3MG36-0AA0","circuit breaker VL400L very high breaking capacity Icu=100kA, 415V AC 3-pole, line protection Electronic Trip Unit ETU22, LSIG 3 phases/3 lines In=315A, rated current IR=128...315A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection without auxiliary release ETU communication-capable without auxiliary/alarm switch",2598,"ST",null,"LP",6.12,1,"3VL47313MG360AA0"]
["3VL4740-1DE36-2HD1","circuit breaker VL400N standard breaking capacity Icu=55kA, 415V AC 3-pole, non-auto. air circ. br. trip unit magnetic In=400A, rated current II=4000A, short-circuit protection Undervoltage release 220...250 V AC Auxiliary/alarm switch mounting kit 2 AUX (1 NO+1 NC)+1 AS (1 NO)","On Request","ST",null,"LP",5.7,1,"3VL47401DE362HD1"]
["3VL4740-2SG36-0AA0","circuit breaker VL400H high breaking capacity Icu=70kA, 415V AC 3-pole, line protection trip unit ETU22, LSIG 3 phases/3 lines In=400A, rated current IR=160...400A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection without auxiliary release without auxiliary/alarm switch",2012,"ST",null,"LP",6.3559999999999999,1,"3VL47402SG360AA0"]
["3VL4840-3VM30-0AA0","circuit breaker VL400X UL type LG (cat no. LLK3G400) non-interchangeable frame, with circuit breaker approval acc. to UL 489 very high breaking capacity 3-pole; NEMA rating 100kA/480V and 18kA/600V (molded case circuit breaker) trip unit LCD ETU, LSIG TA=40Β°C 3 phases/4 lines In=400A, rated current ISD=1.25-10xIR, II=11X in short-circuit protection IR=150-400A ETU for line protection without connection accessories without auxiliary release without auxiliary/alarm switch",7031,"ST",null,"LP",5.9,1,"3VL48403VM300AA0"]
["3VL5750-1EJ46-0AC1","circuit breaker VL630N standard breaking capacity Icu=55kA, 415V AC 4-pole, line protection trip unit TM, LI In=500A, rated current IR=400...500A, overload protection, II=2500...5000A, short-circuit protection N unprotected without auxiliary release Auxiliary switch mounting kit 4 AUX (2 NO + 2 NC)","On Request","ST",null,"LP",11.2,1,"3VL57501EJ460AC1"]
["3VL5750-3DC36-0AA0","circuit breaker VL630L very high breaking capacity Icu=100kA, 415V AC 3-pole, line protection trip unit TM, LI In=500A, rated current IR=400...500A, overload protection, II=2500...5000A, short-circuit protection without auxiliary release without auxiliary/alarm switch",2489,"ST",null,"LP",9.2460000000000004,1,"3VL57503DC360AA0"]
["3VL5763-2DE36-2KA0","circuit breaker VL630H high breaking capacity Icu=70kA, 415V AC 3-pole, non-auto. air circ. br. trip unit magnetic In=630A, rated current II=6300A, short-circuit protection Undervoltage release 440...480 V AC without auxiliary/alarm switch","On Request","ST",null,"LP",9,1,"3VL57632DE362KA0"]
["3VL5763-3LA46-0AA0","circuit breaker VL630L very high breaking capacity Icu=100kA, 415V AC 4-pole, line protection trip unit ETU10, LI In=630A, rated current IR=252...630A, overload protection, II=1.25 to 10xIN, short-circuit protection N protected shipbuilding certificate for LRS, DNV and gL without auxiliary release without auxiliary/alarm switch",5210,"ST",null,"LP",12.18,1,"3VL57633LA460AA0"]
["3VL6180-1KN30-0AA0","circuit breaker VL800 UL; type MG (cat no. NMX3B800) non-interchangeable frame, with circuit breaker approval acc. to UL 489 standard breaking capacity 3-pole, NEMA rating 35kA/480V, (molded case circuit breaker) trip unit TM, LI TA=40Β°C In=< 800A, rated current II=3250...6500A short-circuit protection IR=800A ETU for line protection without connection accessories without auxiliary release without auxiliary/alarm switch",3482,"ST",null,"LP",14,1,"3VL61801KN300AA0"]
["3VL6780-2NF46-0AA0","circuit breaker VL800H high breaking capacity Icu=70kA, 415V AC 4-pole, line protection trip unit ETU20, LSI In=800A, rated current IR=320...800A, overload protection, ISD=1.5 to 7 xIR, II=8 xIN short-circuit protection N protected without auxiliary release ETU communication-capable without auxiliary/alarm switch",3591,"ST",null,"LP",21.56,1,"3VL67802NF460AA0"]
["3VL7112-2VM30-0AA0","circuit breaker VL1200 UL type NG (cat no. HNX3G120) non-interchangeable frame, with circuit breaker approval acc. to UL 489 high breaking capacity 3-pole; NEMA rating 65kA/480V and 35kA/600V (molded case circuit breaker) trip unit LCD ETU, LSIG TA=40Β°C 3 phases/4 lines In=1200A, rated current ISD=1.25-10xIR, II=10xIN short-circuit protection IR=400-1200A overcurrent rel. for line protection without auxiliary release without auxiliary/alarm switch",9199,"ST",null,"LP",25,1,"3VL71122VM300AA0"]
["3VL7180-3VJ30-0AA0","circuit breaker VL1200 UL type NG (cat no. LNX3K800) non-interchangeable frame, with circuit breaker approval acc. to UL 489 very high breaking capacity 3-pole; NEMA rating 100kA/480V and 65kA/600V (molded case circuit breaker) trip unit LCD ETU, LSIG-G with alarm TA=40Β°C 3 phases/4 lines In=800A, rated current ISD=1.25-10xIR, II=8xIN short-circuit protection IR=300-800A ETU for line protection without auxiliary release without auxiliary/alarm switch",10066,"ST",null,"LP",25,1,"3VL71803VJ300AA0"]
["3VL7712-1ME36-0AA0","circuit breaker VL1250N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection trip unit ETU20, LSI In=1250A, rated current IR=500...1250A, overload protection, ISD=1.5 to 9xIR, II=10xIN short-circuit protection without auxiliary release ETU communication-capable without auxiliary/alarm switch",3637,"ST",null,"LP",42,1,"3VL77121ME360AA0"]
["3VL7712-2AA46-0AA0","circuit breaker VL1250H w/o Electronic Trip Unit high breaking capacity Icu=70kA/415V AC, 4-pole In=< 1250A, rated current without auxiliary release with screw terminal connections for switching unit and ETU",2412,"ST",null,"LP",28.25,1,"3VL77122AA460AA0"]
["3VL8112-2VH30-0AA0","circuit breaker VL1600 UL type PG (cat no. HPX3A120) non-interchangeable frame, with circuit breaker approval acc. to UL 489 high breaking capacity 3-pole; NEMA rating 65kA/480V and 35kA/600V (molded case circuit breaker) trip unit LCD ETU, LI/LS/LSI TA=40Β°C In=1200A, rated current ISD=1.25-10xIR, II=10xIN short-circuit protection IR=400-1200A overcurrent rel. for line protection without auxiliary release without auxiliary/alarm switch",12782,"ST",null,"LP",31.3,1,"3VL81122VH300AA0"]
["3VL8716-1SE30-8TE1","circuit breaker VL1600N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection trip unit ETU20, LSI In=1600A, rated current IR=640...1600A, overload protection, ISD=1.5 to 8 xIR, II=9 xIN short-circuit protection Shunt release 208...277 V AC Auxiliary/alarm switch mounting kit 2 AUX (1 NO+1 NC)+1 AS (1 NO)","On Request","ST",null,"LP",33.32,1,"3VL87161SE308TE1"]
["3VL9000-8AU00","accessory for VL160, VL250, VL400, VL630, VL800, VL1250, VL1600 COM20 module for connecting SENTRON VL to Profibus DP reading of measured and parameter values and signals, status of switching func. via motor, with DPV1 functionality",866,"ST",null,"LP",0.28699999999999998,1,"3VL90008AU00"]
["3VL9130-4TD31","accessory for VL150XUL, (CG frame) circular conductor terminal (DELETE) for Cu/Al comprises 3 connections 3-pole only for 60-150A cat. no. 3TA1CG30",81.8,"ST",null,"LP",9.2999999999999999E-2,1,"3VL91304TD31"]
["3VL9200-4TC30","accessory for VL160, box terminals comprises 3 box terminals 3-pole",24.200000000000003,"ST",null,"LP",0.122,1,"3VL92004TC30"]
["3VL9210-6MP30","ETU VL160 3-pole, motor/generator prot. ETU10M, LI IR=40...100A, overload protection, II=1.25 to 11xIN, short-circuit protection box terminal/screw terminal connections in terminal connections in scope of supply of sw. unit",491,"ST",null,"LP",0.99,1,"3VL92106MP30"]
["3VL9216-6UM30","ETU VL160, 3-pole, line protection LCD ETU42, LSIG 3 phases/4 lines with connecting cable IR=64...160A, overload protection, ISD=1.5 to 10xIR, II=11 xIN short-circuit protection box terminal/screw terminal connections in scope of supply of sw. unit",1364,"ST",null,"LP",1.05,1,"3VL92166UM30"]
["3VL9300-4PJ00","accessory for VL160X, VL160, VL250, aux. circuit plug connection for plug-in base",62.7,"ST",null,"LP",0.19600000000000001,1,"3VL93004PJ00"]
["3VL9300-8CA31","accessory for VL150XUL-VL250UL, (CG frame FG frame) terminal cover IP30, extended, comprises 2 covers 3-pole",53.3,"ST",null,"LP",0.30599999999999999,1,"3VL93008CA31"]
["3VL9325-6TF40","ETU VL250 4-pole, line protection ETU20, LSI IR=100...250A, overload protection, ISD=1.5 to 10xIR, II=11 xIN short-circuit protection, N protected screw terminal connections in scope of delivery of switching unit",1320,"ST",null,"LP",0.92,1,"3VL93256TF40"]
["3VL9400-1US01","accessory for VL150XUL, VL150UL VL250UL, VL400UL, VL400XUL (CG frame β€“ LG frame) undervoltage release 220...250V DC f. inst. in r.h. access. comp.",210,"ST",null,"LP",0.105,1,"3VL94001US01"]
["3VL9400-4PS40","accessory for VL400, blade contact kit 4P comprises 8 blade contacts and 1 trip pin",368,"ST",null,"LP",1.744,1,"3VL94004PS40"]
["3VL9400-4WC40","accessory for VL400, withdr. vers., assembly kit front connection, 4-pole",1365,"ST",null,"LP",14.24,1,"3VL94004WC40"]
["3VL9440-6NB40","ETU VL400, 4-pole, line protection ETU10, LI IR=160...400A, overload protection, II=1.25 to 11xIN, short-circuit protection, screw terminal connections in scope of delivery of switching unit",1219,"ST",null,"LP",2.11,1,"3VL94406NB40"]
["3VL9460-4TY33","Breaker LG LUGS Kit OF 3 Power",277,"ST",null,"LP",0.83199999999999996,1,"3VL94604TY33"]
["3VL9600-3HG06","accessory for VL800UL, (MG frame) door op. mech. 8UC7 new design handle red/blue-green, basic masking plate, light gray f. inst. in doors, compl.",283,"ST",null,"LP",1.8,1,"3VL96003HG06"]
["3VL9600-3MM00","accessory for VL630, VL800, mot. op. mech. w/ strd en. mech 220...250V AC/DC with auxiliary switch",1515,"ST",null,"LP",5.66,1,"3VL96003MM00"]
["3VL9710-6LB30","ETU VL1250, 3-pole, line protection ETU10, LI IR=400...1000A, overload protection, II=1.25 to 11xIN, short-circuit protection screw terminal connections in scope of delivery of switching unit shipbuilding certificate for LRS, DNV and gL",2617,"ST",null,"LP",4.25,1,"3VL97106LB30"]
["3VL9712-6LB30","ETU VL1250, 3-pole, line protection ETU10, LI IR=500...1250A, overload protection, II=1.25 to 10xIN, short-circuit protection screw terminal connections in scope of delivery of switching unit shipbuilding certificate for LRS, DNV and gL",3215,"ST",null,"LP",4.25,1,"3VL97126LB30"]
["3VL9800-1SR01","accessory for VL800UL, VL1200UL, VL1600UL, shunt release 110...127V AC for installation on right",223,"ST",null,"LP",0.153,1,"3VL98001SR01"]
["3VL9800-4RH40","accessory for VL1600, flat connecting bars comprises 4 connections 4-pole",247,"ST",null,"LP",6.1050000000000004,1,"3VL98004RH40"]
["3VL9816-6LB30","ETU VL1600, 3-pole, line protection ETU10, LI IR=640...1600A, overload protection, II=1.25 to 9 xIN, short-circuit protection screw terminal connections in scope of delivery of switching unit shipbuilding certificate for LRS, DNV and gL",4573,"ST",null,"LP",4.3449999999999998,1,"3VL98166LB30"]
["3VT1716-2EG46-0AA0","circuit breaker 3VT1 standard breaking capacity Icu=25kA, 415V AC 4-pole; starter combination trip unit TM, LIN In=160A rated current II=800...1600A, short-circuit protection N conductor protected without auxiliary release without auxiliary/alarm switch",412,"ST",null,"LP",1.405,1,"3VT17162EG460AA0"]
["3VT9100-1UC00","accessory for VT160 undervoltage release for 24; 48V AC for mounting on left",96.8,"ST",null,"LP",9.5000000000000001E-2,1,"3VT91001UC00"]
["3VT9300-2AG20","accessory for VT250, VT630 auxiliary switch 2NO 5-60V AC/DC",22.900000000000002,"ST",null,"LP",4.7E-2,1,"3VT93002AG20"]
["3VT9300-4EE30","accessory for VT630, front connecting bars increased pole spacing comprises 3 connections, long 3-pole",64.099999999999994,"ST",null,"LP",0.65100000000000002,1,"3VT93004EE30"]
["3WL1106-2BB32-4GN2","fixed-mounted circuit breaker 3-pole, size I, IEC In=630A to 690V, AC50/60Hz Icu=55kA at 500V rear connection horizontal Overcurrent release ETU 15 LI protection adjustable 0.5-1 in Motorized/manual operating mechanism with spring charging motor AC 50/60 Hz 208-240 V or 220-250 V DC Activation AC 50/60 Hz 230 V, 220 V DC With 1st auxiliary release Shunt release \"F\", F1 50/60 Hz 230 V AC/220 V DC, 100% on-load factor With 2nd auxiliary release \"R\", F3 Undervoltage, instant. 208-240 V AC, 220-250 V DC 2NO+2NC","On Request","ST",1,"LP",43,1,"3WL11062BB324GN2"]
["3WL1108-2CB34-1AA2","fixed-mounted circuit breaker 3-pole, size I, IEC In=800A to 690V, AC50/60Hz Icu=55kA at 500V frnt.conn. top/bot. dual-hole Overcurrent release ETU 25 LSI protection adjustable 0.4-1 in With manual operating mechanism with storage with mechanical request without 1st auxiliary release without 2nd auxiliary release 2NO+2NC","On Request","ST",1,"LP",43,1,"3WL11082CB341AA2"]
["3WL1116-2BB32-1AN2","fixed-mounted circuit breaker 3-pole, size I, IEC In=1600A to 690V, AC50/60Hz Icu=55kA at 500V rear connection horizontal Overcurrent release ETU 15 LI protection adjustable 0.5-1 in With manual operating mechanism with storage with mechanical request without 1st auxiliary release With 2nd auxiliary release \"R\", F3 Undervoltage, instant. 208-240 V AC, 220-250 V DC 2NO+2NC","On Request","ST",1,"LP",52,1,"3WL11162BB321AN2"]
["3WL1116-3EB32-4GN4","fixed-mounted circuit breaker 3-pole, size I, IEC In=1600A to 690V, AC50/60Hz Icu=66kA at 500V rear connection horizontal Overcurrent release ETU 45 LSIN protection adjustable 0.4-1 in with cubicle bus Opt.: Comm. /measuring func./ground fault/ ZSS Motorized/manual operating mechanism with spring charging motor AC 50/60 Hz 208-240 V or 220-250 V DC Activation AC 50/60 Hz 230 V, 220 V DC With 1st auxiliary release Shunt release \"F\", F1 50/60 Hz 230 V AC/220 V DC, 100% on-load factor With 2nd auxiliary release \"R\", F3 Undervoltage, instant. 208-240 V AC, 220-250 V DC 4NO+4NC","On Request","ST",1,"LP",43,1,"3WL11163EB324GN4"]
["3WL1225-2CB35-1AA2","withdrawable circuit breaker without guide frame 3-pole, size II, IEC In=2500A to 690V, AC50/60Hz Icu=66kA at 500V rear connection horizontal Overcurrent release ETU 25 LSI protection adjustable 0.4-1 in With manual operating mechanism with storage with mechanical request without 1st auxiliary release without 2nd auxiliary release 2NO+2NC","On Request","ST",1,"LP",63,1,"3WL12252CB351AA2"]
["3WL1225-4CB38-1AA2","withdrawable circuit breaker with guide frame 3-pole, size II, IEC In=2500A to 690V, AC50/60Hz Icu=100kA at 500V w. connection flange Overcurrent release ETU 25 LSI protection adjustable 0.4-1 in With manual operating mechanism with storage with mechanical request without 1st auxiliary release without 2nd auxiliary release 2NO+2NC","On Request","ST",1,"LP",102,1,"3WL12254CB381AA2"]
["3WL9111-0AD01-0AA0","accessories circuit breaker 3WL shunt trip DC 24V, 100% ed",196,"ST",null,"LP",0.7,1,"3WL91110AD010AA0"]
["3WL9111-0AH02-0AA0","accessories circuit breaker 3WL signal switch for 1st and  2nd aux. release",48.1,"ST",null,"LP",0.02,1,"3WL91110AH020AA0"]
["3WL9111-0AS02-0AA0","accessories circuit breaker 3WL arc chute size II, for 690V",72.099999999999994,"ST",null,"LP",1.68,1,"3WL91110AS020AA0"]
["3WL9111-0BA22-0AA0","accessories circuit breaker 3WL prot.cover f. mech. on/off safety lock ces",267,"ST",null,"LP",0.51200000000000001,1,"3WL91110BA220AA0"]
["3WL9111-1AT16-0AA0","3WL9 NAFTA accessory WLBSS BSS (breaker status sensor)",3409,"ST",null,"LP",0.13700000000000001,1,"3WL91111AT160AA0"]
["3WL9212-3AC40-1AA1","Accessory f. breaker 3WL guide frame  size II 2000A 3-pole, rear horizontal connection With 4 auxiliary plug connectors without auxiliary current plug connectors With 3 change-over contacts, Operation 1 CO, Test 1 CO, Isolated position 1 CO without shutter","On Request","ST",1,"LP",31,1,"3WL92123AC401AA1"]
["3WL9327-7AA00-0AA1","3WL9-NAFTA accessories ETU776G WLETU776G Protection function LSIG",22176,"ST",null,"LP",0.75,1,"3WL93277AA000AA1"]
["4RF5605-3EA47","5.67% choked capacitor module for cabinet width 800 mm for cabinet depth 400 mm with MKK capacitors with discharge unit with fuse Switch disconnector fronts. Busbar 30x 10 mm 50kVAr 400V 50Hz can be switched as 1x 50 kVAr","On Request","ST",null,"LP",52,1,"4RF56053EA47"]
["5SD603","DIAZED fuse link 750 V DC rail system protection Quick-response characteristic size DIII, E33, 6A",9.48,"ST",null,"LP",7.0000000000000007E-2,5,"5SD603"]
["5SF1024","DIAZED base DII 25 A 500 V AC DC 500 V AC DC for screw mounting","On Request","ST",1,"LP",9.9000000000000005E-2,5,"5SF1024"]
["5SH5025","NEOZED adapter sleeve D02 25 A",0.47000000000000003,"ST",null,"LP",8.0000000000000004E-4,50,"5SH5025"]
["5SJ6520-7KS","Miniature circuit breaker 230 V 6kA, 1+N-pole, C, 20 A, D=70 mm with screwless outgoing terminals",12.299999999999999,"ST",null,"LP",0.218,1,"5SJ65207KS"]
["5SL3106-7","Miniature circuit breaker 230/400 V 4.5 kA, 1-pole, C, 6A",5.42,"ST",null,"LP",0.13200000000000001,1,"5SL31067"]
["5SL3663-6","Miniature circuit breaker 400 V 4.5 kA, 3+N-pole, B, 63 A",43.4,"ST",null,"LP",0.66,1,"5SL36636"]
["5SL4116-7","Miniature circuit breaker 230/400 V 10kA, 1-pole, C, 16A",9.0299999999999994,"ST",null,"LP",0.152,1,"5SL41167"]
["5SL4340-8","Miniature circuit breaker 400 V 10kA, 3-pole, D, 40 A",114,"ST",null,"LP",0.46400000000000002,1,"5SL43408"]
["5SL4450-6","Miniature circuit breaker 400 V 10kA, 4-pole, B, 50 A",79.599999999999994,"ST",null,"LP",0.64200000000000002,1,"5SL44506"]
["5SL6103-7","Miniature circuit breaker 230/400 V 6kA, 1-pole, C, 3A",8.93,"ST",null,"LP",0.124,1,"5SL61037"]
["5SL6301-7","Miniature circuit breaker 400 V 6kA, 3-pole, C, 1 A",34.6,"ST",null,"LP",0.44900000000000001,1,"5SL63017"]
["5SL6406-6","Miniature circuit breaker 400 V 6kA, 4-pole, B, 6A",31.6,"ST",null,"LP",0.49399999999999999,1,"5SL64066"]
["5SM1616-0","Residual current operated circuit breaker, 2-pole, type AC, In: 63 A, 300 mA, Un AC: 230 V","On Request","ST",null,"LP",0.29299999999999998,1,"5SM16160"]
["5SM2626-6","RC unit for 5SL4, 2-pole, type A, In: 63 A, 300 mA, Un AC: 230 V",109,"ST",null,"LP",0.192,1,"5SM26266"]
["5SM3444-0","Residual current operated circuit breaker, 4-pole, type AC, In: 40 A, 100 mA, Un AC: 400 V","On Request","ST",1,"LP",0.47199999999999998,1,"5SM34440"]
["5SP3740","Main miniature circuit breaker (SHU), selective, 1-pole, 40A","On Request","ST",null,"LP",0.47299999999999998,1,"5SP3740"]
["5SP4492-6","Miniature circuit breaker 400 V 10kA, 4-pole, B, 125 A, D=70 mm",286,"ST",null,"LP",1.0660000000000001,1,"5SP44926"]
["5ST2140","Busbar, touch-safe for N miniature circuit breaker 5SX 210 mm long with end caps for 12 MW, 10 mm2 CU, 3-phase","On Request","ST",null,"LP",0.11,1,"5ST2140"]
["5ST3011","Auxiliary current switch 2 NO for circuit breaker 5SL, 5SY, 5SP Incorporated switch 5TL1, RCBO 5SU1, FI 5SV (for 5SU1 handle coupler 5ST3805-1 is required)",13.2,"ST",null,"LP",6.5000000000000002E-2,1,"5ST3011"]
["5ST3602","Pin busbar, 10 mm2 connection: 12x 1-phase touch-safe",2.7199999999999998,"ST",null,"LP",4.7E-2,10,"5ST3602"]
["5ST3763","Pin busbar, 1-phase 10 mm2, 12 pins, Insulation blue can be cut, with end caps",5.09,"ST",null,"LP",3.4000000000000002E-2,10,"5ST3763"]
["5SU1324-7FA20","RCBO, 10 kA, 2P, type A, 30 mA, C-Char, In: 20 A, Un AC: 230 V",207,"ST",null,"LP",0.41199999999999998,1,"5SU13247FA20"]
["5SU1356-7KK20","RCBO, 6 kA, 1P+N, type A, 30 mA, C-Char, In: 20 A, Un AC: 230 V",156,"ST",null,"LP",0.28000000000000003,1,"5SU13567KK20"]
["5SU1656-6KK32","RCBO, 6 kA, 1P+N, type A, 300 mA, B char., In: 32 A, Un AC: 230 V",139,"ST",null,"LP",0.28199999999999997,1,"5SU16566KK32"]
["5SV3344-3","Residual current operated circuit breaker, 4-pole, type F, short-time delayed, In: 40 A, 30 mA, Un AC: 400 V",254,"ST",null,"LP",0.38700000000000001,1,"5SV33443"]
["5SV3617-6","Residual current operated circuit breaker, 2-pole, type A, In: 80 A, 300 mA, Un AC: 230 V",194,"ST",null,"LP",0.20399999999999999,1,"5SV36176"]
["5SV4614-0KL","Residual current operated circuit breaker, 2-pole, Type AC, In: 40 A, 300 mA, Un AC: 230 V, N left",59.5,"ST",null,"LP",0.185,1,"5SV46140KL"]
["5SW3010","Terminal cover for residual current operated circuit breaker 5SM1 2 MW",4.76,"ST",null,"LP",1.2E-2,1,"5SW3010"]
["5SY3350-7","CIRCUIT BREAKER 400V 4.5KA, 3-POLE, C, 50A, D=70MM","On Request","ST",1,"LP",0.48699999999999999,1,"5SY33507"]
["5SY4125-5","Miniature circuit breaker 230/400 V 10kA, 1-pole, A, 25A, D=70 mm",26.700000000000003,"ST",null,"LP",0.16400000000000001,1,"5SY41255"]
["5SY4163-8","Miniature circuit breaker 230/400 V 10kA, 1-pole, D, 63 A, D=70 mm",56.4,"ST",null,"LP",0.16600000000000001,1,"5SY41638"]
["5SY4308-5","Miniature circuit breaker 400 V 10kA, 3-pole, A, 8A, D=70 mm",130,"ST",null,"LP",0.46700000000000003,1,"5SY43085"]
["5SY4320-6KK11","Miniature circuit breaker 400 V 10kA, 3-pole, B, 20A for railway applications","On Request","ST",null,"LP",0.46100000000000002,1,"5SY43206KK11"]
["5SY4410-6","Miniature circuit breaker 400 V 10kA, 4-pole, B, 10A, D=70 mm",53.2,"ST",null,"LP",0.61299999999999999,1,"5SY44106"]
["5SY4513-5","Miniature circuit breaker 230 V 10kA, 1+N-pole, A, 13 A, D=70 mm",51.2,"ST",null,"LP",0.32400000000000001,1,"5SY45135"]
["5SY5105-7","Circuit breaker Universal current 220 V DC 230/400 V AC 10kA, 1-pole, C, 0.5 A",19.3,"ST",null,"LP",0.17100000000000001,1,"5SY51057"]
["5SY5204-7KK11","Circuit breaker Universal current 440 V DC/400 V AC 10kA, 2-pole, C, 4 A for railway applications","On Request","ST",null,"LP",0.318,1,"5SY52047KK11"]
["5SY6040-6","Miniature circuit breaker 230 V 6kA, 1+N-pole/1 MW, B 40 A",25.5,"ST",null,"LP",0.126,1,"5SY60406"]
["5SY6150-6","Miniature circuit breaker 230/400 V 6kA, 1-pole, B, 50 A, D=70 mm",17.3,"ST",null,"LP",0.16900000000000001,1,"5SY61506"]
["5SY6413-7","Miniature circuit breaker 400 V 6kA, 4-pole, C, 13 A, D=70 mm",47.9,"ST",null,"LP",0.624,1,"5SY64137"]
["5SY7110-8","Miniature circuit breaker 230/400 V 15kA, 1-pole, D, 10A, D=70 mm",27.8,"ST",null,"LP",0.157,1,"5SY71108"]
["5SY7332-8","Miniature circuit breaker 400 V 15kA, 3-pole, D, 32 A, D=70 mm",134,"ST",null,"LP",0.48,1,"5SY73328"]
["5SY7463-8","Miniature circuit breaker 400 V 15kA, 4-pole, D, 63 A, D=70 mm",326,"ST",null,"LP",0.65400000000000003,1,"5SY74638"]
["5SY8114-7","Circuit breaker 230/400 V D=70 mm 25 kA according to EN 60947-2, 1P, C0.3",19.3,"ST",null,"LP",0.16500000000000001,1,"5SY81147"]
["5SY8263-7","Miniature circuit breaker 400 V D=70 mm 25 kA according to EN 60947-2, 2P, C63",93.5,"ST",null,"LP",0.34399999999999997,1,"5SY82637"]
["5SY8320-7","Miniature circuit breaker 400 V D=70 mm 25 kA according to EN 60947-2, 3P, C20",64.099999999999994,"ST",null,"LP",0.46700000000000003,1,"5SY83207"]
["5SY8606-8","Miniature circuit breaker 400 V D=70 mm 25 kA according to EN 60947-2, 3P+N, D6",183,"ST",null,"LP",0.60899999999999999,1,"5SY86068"]
["5TA2162-0KK","DELTA switch device insert FM, OFF switch 2-pole without claws 10A 250V",29.8,"ST",null,"LP",4.7E-2,10,"5TA21620KK"]
["5TC1532","DELTA i-system electrical white Sun-blind control Complete unit, 55x 55 mm",213,"ST",null,"LP",0.19700000000000001,1,"5TC1532"]
["5TD2813","DELTA i-system titanium white Light signal 250 V with glow lamp Cover plate 55x 55 m with red window",29.200000000000003,"ST",null,"LP",7.6999999999999999E-2,1,"5TD2813"]
["5TE6801","SCHUKO socket outlet 16 A with cover according to DIN VDE 0620 for installation in distribution boards",9.0499999999999989,"ST",null,"LP",9.0999999999999998E-2,1,"5TE6801"]
["5TE8311","SWITCH, D=70MM 32A 1NC, TERMINAL 50QMM","On Request","ST",1,"LP",0.11,1,"5TE8311"]
["5TG1204-0","DELTA miro Frame 4-fold Authentic material glass crystal green without Siemens logo Dimensions 303x 90 mm",191,"ST",null,"LP",0.47299999999999998,1,"5TG12040"]
["5TG1260","DELTA i-system aluminum-metallic Cover plate UAE connection socket suitable for Ackermann Cat. 3 1x 8-pole, 55x 55 mm",13.299999999999999,"ST",null,"LP",7.0000000000000001E-3,1,"5TG1260"]
["5TG1825","DELTA profil, titanium white Surface-mounting enclosure, 1 x 80x 80x 42.5 mm",18.3,"ST",null,"LP",7.6999999999999999E-2,1,"5TG1825"]
["5TG2078","Support plate red insert for accommodating up to 2 modular jack connectors Screw mounting PEHA design. MJ1",7.87,"ST",null,"LP",3.4000000000000002E-2,1,"5TG2078"]
["5TG4205","DELTA flaeche IP44, AP) Slide nipple for cable entry for connection of single devices with hole",1.71,"ST",null,"LP",0.01,1,"5TG4205"]
["5TG5507-4KK","CORAL, IRIS, MEGA Video connection socket 1 compartment",57.9,"ST",null,"LP",5.0999999999999997E-2,1,"5TG55074KK"]
["5TG5522-3LG","CORAL Frame 3-fold, horizontal lava grey","On Request","ST",1,"LP",7.4999999999999997E-2,1,"5TG55223LG"]
["5TG5523-1WH","CORAL Frame 3-fold, horizontal with intermediate frames polar white","On Request","ST",1,"LP",7.2999999999999995E-2,1,"5TG55231WH"]
["5TG5524-5MS","CORAL Cover plate for Loudspeaker Potentiometers moon silver","On Request","ST",1,"LP",3.5999999999999997E-2,1,"5TG55245MS"]
["5TG5532-4DG","IRIS Cover plate for Socket outlet with spring flap and child protection sand gold","On Request","ST",null,"LP",3.7999999999999999E-2,1,"5TG55324DG"]
["5TG5534-6BE","IRIS Frame 3-fold, vertical beige","On Request","ST",null,"LP",4.2000000000000003E-2,1,"5TG55346BE"]
["5TG5930-2MA","IRIS Water sensor Mercury aluminum","On Request","ST",null,"LP",0.13600000000000001,1,"5TG59302MA"]
["5TG6224","DELTA i-system carbon metallic Rocker switch with window for Series/double two-way switch 55x 55 mm",7.09,"ST",null,"LP",2.3E-2,1,"5TG6224"]
["5TG7802","DELTA profil, titanium white Rocker switch with symbols I0 for OFF switch 2-pole, 3-pole 65x 65 mm",8.99,"ST",null,"LP",2.5000000000000001E-2,1,"5TG7802"]
["5TG8065","Cap set for button 5TE48 Set with 5x each/black /non-transparent",9.1,"SZ",null,"LP",1E-3,1,"5TG8065"]
["5TT3441","Soft starting device T5570 400 V AC 1600W 1PH With transparent cap","On Request","ST",1,"LP",0.13700000000000001,1,"5TT3441"]
["5TT4201-3","switching relay with 1 NO contact for 230V AC 16A control 12V AC",41.1,"ST",null,"LP",0.126,1,"5TT42013"]
["5TT5842-2","INSTA contactor with 2 NO contact and 2 NC contacts Contact for 230 V AC, 400V 40A Control 24 V AC",86.699999999999989,"ST",null,"LP",0.39400000000000002,1,"5TT58422"]
["5TT6114","overcurrent relay T5570 230V AC 1/5/10/15A 1-phase with transparent cap",239,"ST",null,"LP",0.14899999999999999,1,"5TT6114"]
["5UB1916","DELTA i-system titanium white SCHUKO socket outlet 10/16 A 250 V With screwless Connection terminals with increased touch protection w. spring flap 55x 55 mm, with lock",43.4,"ST",null,"LP",0.124,1,"5UB1916"]
["5UB1998-0KF","Promotional package DELTA i-system",863,"ST",null,"LP",8.6519999999999992,1,"5UB19980KF"]
["5UB5530-5DG","IRIS SCHUKO socket outlet 10/16 A 250 V Operating display Cover plate odyssey gold with increased touch protection child protection",25.1,"ST",null,"LP",7.0999999999999994E-2,1,"5UB55305DG"]
["7KT1652","SENTRON, measuring device, 7KT PAC1600, LCD, L-N: 230 V, 63 A, strd rail instr., sing.-ph., Modbus RTU/ASCII + MID, app. /active/reactive energy, self-powered, screw terminals",179,"ST",null,"LP",0.151,1,"7KT1652"]
["8GB2052-2","SIMBOX Universal WP N/PE terminal strip 2x5x 25 mm2+2x14x 10 mm2",23.3,"ST",null,"LP",0.42199999999999999,10,"8GB20522"]
["8GF5681","Stab/SIKUS Universal Copper bar, flexible, L=2000 mm 20x 5x 1 mm 250 A, temp. 20 Β°C",329,"ST",null,"LP",2,1,"8GF5681"]
["8GK1032-5KK41","ALPHA 160, wall-mounted cabinet, IP43, Protection class 2, H: 1100 mm, W: 1050 mm, T: 140 mm, RAL 9016",651,"ST",null,"LP",31,1,"8GK10325KK41"]
["8GK1112-3KK42","ALPHA 400, wall-mounted cabinet, Flat Pack, IP43, Protection class 2, H: 800 mm, W: 1050 mm, T: 210 mm, RAL 9016",539,"ST",null,"LP",27,1,"8GK11123KK42"]
["8GK1122-2KK22","ALPHA 400, wall-mounted cabinet, IP43, Protection class 1, H: 650 mm, W: 550 mm, T: 210 mm, RAL 9016","On Request","ST",1,"LP",12,1,"8GK11222KK22"]
["8GK1312-8KK42","ALPHA 630, Floor-mounted cabinet, Flat Pack, IP43, Protection class 2, H: 1900 mm, W: 1050 mm, T: 210 mm, RAL 7035",1464,"ST",null,"LP",63.5,1,"8GK13128KK42"]
["8GK2420-6KK14","ALPHA 800 UNIVERSAL, Floor-mounted cabinet, IP55, Protection class 1, H: 1800 mm, W: 300 mm, T: 400 mm, RAL 7035, without door",940,"ST",null,"LP",32.299999999999997,1,"8GK24206KK14"]
["8GK4301-4KK11","ALPHA 160 DIN, Mounting kit for modular installation devices, Clearance between rows 125 mm H=600 W=250",113,"ST",null,"LP",0.88700000000000001,1,"8GK43014KK11"]
["8GK4401-3KK22","ALPHA 400/630 DIN, Assembly kit Modular terminal blocks with terminal strip Section cover closed horizontal, H=450 W=500",97.1,"ST",null,"LP",2.0569999999999999,1,"8GK44013KK22"]
["8GK4731-3KK10","ALPHA 400/630 DIN Circuit breaker kit 1x 3VA10-11/100A/160A 3+4-pole H=450 mm W=250 mm, horizontal Installation RCD module laterally mounted",143,"ST",null,"LP",1.7629999999999999,1,"8GK47313KK10"]
["8GK4801-3KK12","ALPHA 400/630 DIN, Assembly kit for busbar-adaptable N-system 3-pole, H=450 W=250 devices on 60 mm busbar",184,"ST",null,"LP",1.357,1,"8GK48013KK12"]
["8GK6715-4KK33","ALPHA 630 Universal, Circuit breaker kit 1x 3VL630, 3+4-pole H=400 mm W=900 mm, horizontal Installation",153,"ST",null,"LP",8.6999999999999993,1,"8GK67154KK33"]
["8GK6740-6KK23","ALPHA 630 Universal Circuit breaker kit 3x 3VA23-24/400A/630A 3+4-pole H=600 mm W=600 mm, vertical installation",149,"ST",null,"LP",8.26,1,"8GK67406KK23"]
["8GK9400-0KK45","ALPHA 1600 DIN, Adapter set for modular distribution board H=2000 W=1100 D=400",249,"SZ",null,"LP",12,1,"8GK94000KK45"]
["8GK9510-8KK20","ALPHA, door, on the right, IP55, H: 1250 mm, W: 550 mm, RAL 9016, type of protection 1 and 2",164,"ST",null,"LP",7.3920000000000003,1,"8GK95108KK20"]
["8GK9533-0KK10","ALPHA, mounting plate, H: 1800 mm, W: 250 mm",113,"ST",null,"LP",6.5,1,"8GK95330KK10"]
["8GK9607-2KK10","ALPHA 630 Universal, Section cover without cutouts H=400 mm, W=300 mm",53.4,"ST",null,"LP",1.2809999999999999,1,"8GK96072KK10"]
["8GK9608-3KK22","ALPHA 630 Universal, Section cover with cutouts 3x 24 MW, Clearance between rows 150 mm H=450 mm W=600 mm",92.899999999999991,"ST",null,"LP",2.0699999999999998,1,"8GK96083KK22"]
["8GK9910-0KK27","ALPHA DIN assembly tool for Support, short and long version with ergonomic handle shape",69.8,"ST",null,"LP",0.26800000000000002,1,"8GK99100KK27"]
["8GK9920-0KK25","ALPHA 630 Universal, 1 set of replacement hinges for section cover consisting of 6 units with fixing accessories",23.400000000000002,"SZ",null,"LP",0.26,1,"8GK99200KK25"]
["8MF1000-2HA","SIVACON, earthquake kit",693,"ST",null,"LP",8,1,"8MF10002HA"]
["8MF1006-2VB","SIVACON, Roof tray rim, for cabinet side IPX1, T: 600 mm, RAL 7035",86.5,"ST",null,"LP",2,1,"8MF10062VB"]
["8MF1024-2UD30-0A","SIVACON, Roof, with Ventilation openings with Ventilation openings IP40, W: 1200 mm, T: 400 mm, zinc-plated",84.6,"ST",null,"LP",6,1,"8MF10242UD300A"]
["8MF1028-2UD10-0A","SIVACON, Roof, Closed, IP40, W: 1200 mm, T: 800 mm, zinc-plated",110,"ST",null,"LP",11.65,1,"8MF10282UD100A"]
["8MF1066-2UD10-0A","SIVACON, Roof, Closed, IP40, W: 600 mm, T: 600 mm, zinc-plated",57.6,"ST",null,"LP",4.5999999999999996,1,"8MF10662UD100A"]
["8MF1070-2UT14-0BA2","SIVACON, door, right, IP55, H: 2000 mm, W: 450 mm, RAL 7035, Protection class 1",405,"ST",null,"LP",12.93,1,"8MF10702UT140BA2"]
["8MF1088-2UB22-0","SIVACON, base, IP30, D: 800 mm, W: 800 mm, zinc-plated",100,"ST",null,"LP",8.5,1,"8MF10882UB220"]
["8MF1096-2UB42-0","SIVACON, base, EMC, IP40, D: 600 mm, W: 900 mm, zinc-plated",133,"ST",null,"LP",6.7,1,"8MF10962UB420"]
["8MF1200-3VR4","SIVACON, Control panel Empty enclosure, without side panels, according to IEC 62208, with Ventilation openings IP20, H: 2200 mm, W: 1000 mm, T: 1000 mm",2646,"ST",null,"LP",182,1,"8MF12003VR4"]
["8MF1215-2AS30","SIVACON, mounting rail, L: 2150 mm, zinc-plated",62.9,"ST",null,"LP",3.68,1,"8MF12152AS30"]
["8MF1270-2UT14-0CA1","SIVACON, door, right, EMC, IP40, H: 2200 mm, W: 450 mm, RAL 7035, Protection class 1",828,"ST",null,"LP",14.151,1,"8MF12702UT140CA1"]
["8MF1280-3BR4","SIVACON, Control panel Empty enclosure, without side panels, according to IEC 62208, IP40, H: 2200 mm, W: 800 mm, T: 1000 mm",2049,"ST",null,"LP",154.18,1,"8MF12803BR4"]
["8MF1298-3BS4","SIVACON, Control panel Empty enclosure, according to IEC 62208, IP40, H: 2200 mm, W: 900 mm, T: 800 mm",2977,"ST",null,"LP",208.94,1,"8MF12983BS4"]
["8MF1800-2AN30","SIVACON, cabinet frame, for installation of 19\" devices, H: 2000 mm, zinc-plated",129,"ST",null,"LP",9.1,1,"8MF18002AN30"]
["8MF1880-2UT14-0BE2","SIVACON, door, right, inspection window, IP55, H: 1800 mm, W: 800 mm, RAL 7035, Protection class 1",621,"ST",null,"LP",19,1,"8MF18802UT140BE2"]
["8MF2006-4R","standard cabinet 8MF2 HxWxD=2000x 1000x 600 Installation: Side-by-side non-ventilated, assembled, welded IP40",2928,"ST",null,"LP",145,1,"8MF20064R"]
["8MF2064-4RB","standard cabinet 8MF2 HxWxD=2000x 600x 400 Installation: Side-by-side ventilated, mounted, welded IP40",2231,"ST",null,"LP",105,1,"8MF20644RB"]
["8MF2284-4R","standard cabinet 8MF2 HxWxD=2200x 800x 400 Installation: Side-by-side non-ventilated, assembled, welded IP40",2339,"ST",null,"LP",135,1,"8MF22844R"]
["8MF2296-4R","standard cabinet 8MF2 HxWxD=2200x 900x 600 Installation: Side-by-side non-ventilated, assembled, welded IP40",2524,"ST",null,"LP",165,1,"8MF22964R"]
["8MF2896-5R","standard cabinet 8MF2 HxWxD=1800x 900x 600 Installation: Side-by-side non-ventilated, assembled, welded IP54,",2677,"ST",null,"LP",110,1,"8MF28965R"]
["8MF3066-6","compartment door instead of a standard door HxW=2000x 600",844,"ST",null,"LP",20,1,"8MF30666"]
["8MF3310","Locking handle large without Lock Price is an additional price for Standard version",84.6,"ST",null,"LP",0.125,1,"8MF3310"]
["8MF3438","SIVACON, roof, with ventilation openings IP40, W: 1200 mm, D: 800 mm, RAL 7032",434,"ST",null,"LP",0.1,1,"8MF3438"]
["8MF4020","Socket HxWxD=100x 900x 400",354,"ST",null,"LP",8.1999999999999993,1,"8MF4020"]
["8MF4071","Base plate without subdivision WxD=900x 600",256,"ST",null,"LP",5.694,1,"8MF4071"]
["8MF4500","Mounting plate incl. mounting bracket HxW=1800x 600",309,"ST",null,"LP",22.01,1,"8MF4500"]
["8MF4612","mounting plate HxW=200x 900",127,"ST",null,"LP",10,1,"8MF4612"]
["8MF4896","19-inch swing frame crossbar W=900 consisting of 2 units",586,"ST",null,"LP",9.8030000000000008,1,"8MF4896"]
["8MF5068-4R","Standard cabinet 8MF5 HxWxD=2000x 600x 800 Installation: Side-by-side non-ventilated, not mounted, screwed IP40",2501,"ST",null,"LP",120,1,"8MF50684R"]
["8MF5828-4R","Standard cabinet 8MF5 HxWxD=1800x 1200x 800 Installation: Side-by-side non-ventilated, not mounted, screwed IP40",3505,"ST",null,"LP",135,1,"8MF58284R"]
["8MF5900-3B","SlimLine lamp with On/Off switch SL 025 without socket outlet Solenoid (approx. 30 N)","On Request","ST",null,"LP",0.54100000000000004,1,"8MF59003B"]
["8MF6068-4R","Standard cabinet 8MF6 HxWxD=2000x 600x 800 Installation: Side-by-side non-ventilated, assembled, welded IP40",2501,"ST",null,"LP",120,1,"8MF60684R"]
["8MF6866-4E","Standard cabinet 8MF6 HxWxD=1800x 600x 600 Installation: single non-ventilated, assembled, welded IP40",2854,"ST",null,"LP",90,1,"8MF68664E"]
["8MF9060","Locking bar H=1800",25.3,"ST",null,"LP",0.38,1,"8MF9060"]
["8MR2140-6C","fan heater 230V, 600 W; HV030",365,"ST",null,"LP",0.65500000000000003,1,"8MR21406C"]
["8MR2170-1DB","Thermostat NO contact +20 to 80 Β°C",42.2,"ST",null,"LP",5.8000000000000003E-2,1,"8MR21701DB"]
["8MR6511-5LV25","Filter fan, Extract: W: 125 mm, H: 125 mm, RAL 7035, IP55, Airflow: 58 m3/h, Ue AC: 115 V",304,"ST",null,"LP",0.81399999999999995,1,"8MR65115LV25"]
["8PQ1014-0BA02","SIVACON S4 Base reinforcements Height 100 mm Width, Depth=400 mm",52.9,"ST",null,"LP",1.6220000000000001,1,"8PQ10140BA02"]
["8PQ2000-8BA03","SIVACON S4 Masking frame Equipment height 1600 mm fixed Width 800 mm",162,"ST",null,"LP",10.15,1,"8PQ20008BA03"]
["8PQ2015-6BA35","SIVACON S4, Compartment door, for 3VA molded case circuit breaker with door-coupling rotary operating mechanism, 3VA12 (250 A), horizontal, fixed mounting, Number of switches 1, IP40, H: 150 mm, W: 600 mm, double-bit",70.199999999999989,"ST",null,"LP",2.8,1,"8PQ20156BA35"]
["8PQ2025-8BA13","SIVACON S4 Masking frame SENTRON 3VA 3VA20 (up to 100 A) 3VA21 (up to 160 A) 3VA22 (up to 250 A) 3-pole Mounting position horizontal withdrawable connection Number of switches 1 Height 250 mm Width 800 mm",108,"ST",null,"LP",1.65,1,"8PQ20258BA13"]
["8PQ2035-8BA01","SIVACON S4 Cover Closed Height 350 mm Width 800 mm",57.6,"ST",null,"LP",2.06,1,"8PQ20358BA01"]
["8PQ2055-0BA07","SIKUS/SIVACON Upgrade modular door to degree of protection IP55 Height 550 mm Width 1100 mm",59.9,"ST",null,"LP",1.345,1,"8PQ20550BA07"]
["8PQ2055-8BA13","SIVACON S4 Masking frame SENTRON 3VA 3VA20 (up to 100 A) 3VA21 (up to 160 A) 3VA22 (up to 250 A) 3-pole Upright mounting position Fixed mounting Number of switches 5 Height 550 mm Width 800 mm",132,"ST",null,"LP",3.7,1,"8PQ20558BA13"]
["8PQ2070-6BA04","SIVACON S4 compartment door Upgrade IP55 Height 700 mm Width 600 mm",56.800000000000004,"ST",null,"LP",1.3089999999999999,1,"8PQ20706BA04"]
["8PQ2197-4BA11","SIVACON S4, door, IP40, H: 1975 mm, W: 400 mm, Double-bit, right",220,"ST",null,"LP",13.25,1,"8PQ21974BA11"]
["8PQ2300-6BA02","SIKUS/SIVACON Floor panel with openings for 6 flanges Degree of protection up to IP55 Width 850 mm Depth 600 mm",63.9,"ST",null,"LP",3.41,1,"8PQ23006BA02"]
["8PQ2308-6BA01","SIVACON S4 Top plate Degree of protection IP55 Closed Width 800 mm Depth 600 mm",59.9,"ST",null,"LP",6.1,1,"8PQ23086BA01"]
["8PQ3000-1BA37","SIVACON S4, Section division, 1800 mm, T: 800 mm, zinc-plated",78.8,"ST",null,"LP",6.8,1,"8PQ30001BA37"]
["8PQ3000-2BA06","SIKUS/SIVACON Subdivision shape 2B Main busbar Width 400 mm Depth 600 mm",110,"ST",null,"LP",2.14,1,"8PQ30002BA06"]
["8PQ3000-2BA72","SIVACON S4 Subdivision for the main busbar system Form 2B Main busbar front Width 850 mm Depth 600 mm",126,"ST",null,"LP",9.1999999999999993,1,"8PQ30002BA72"]
["8PQ5000-1BA67","SIVACON S4 Subdivision 3WL Shape 4 Switch 3WL11 630-1000 A 3 or 4-pole Fixed mounting, Insert Distribution busbar connection Height over 3WL 250 mm Height under 3WL 300 mm Width 800 mm Depth 600, 800mm",109,"ST",null,"LP",9.02,1,"8PQ50001BA67"]
["8PQ5000-2BA61","SIVACON S4 Subdivision horizontal Form 3 Width 600 mm",41,"ST",null,"LP",1.96,1,"8PQ50002BA61"]
["8PQ5000-4BA42","SIVACON S4 Subdivision vertical at the back Form 3 Width 600 Height 250",56.3,"ST",null,"LP",1.7629999999999999,1,"8PQ50004BA42"]
["8PQ6000-3BA78","SIVACON S4 EBS SENTRON 3NP Switch 3NP1123 and 1133 Upright mounting position Fixed mounting Number of switches 4 Height 250 mm for 3NP1123 Height 300 mm for 3NP1133 Width 800 mm",52,"ST",null,"LP",2.1,1,"8PQ60003BA78"]
["8PQ6000-5BA01","SIVACON S4 EBS SENTRON 3VL Switch 3VL1 up to 160 A 4-pole Mounting position horizontal Fixed mounting Number of switches 1 Height 200 mm Width 600 mm",43.5,"ST",null,"LP",2.7,1,"8PQ60005BA01"]
["8PQ6000-5BA76","SIVACON S4 EBS holder and drawings for switch connection to cable SENTRON 3WL1116 Fixed-mounted and withdrawable version Width 800 mm for masking frame",458,"ST",null,"LP",7.26,1,"8PQ60005BA76"]
["8PQ6015-8AA88","Basic configuration 100","On Request","ST",null,"LP",1E-3,1,"8PQ60158AA88"]
["8PQ9111-1AA03","Spring 7.27x 31","On Request","ST",{"$f":"#REF!","v":{"$error":"#REF!"}},"LP",2E-3,100,"8PQ91111AA03"]
["8UC6034","Spare part for rotary operating mechanism 8UC6 Extension shaft 300 mm long 12x 12 mm",16.2,"ST",null,"LP",0.316,1,"8UC6034"]
["8UC9385","Operating mechanism for fixed mounting for switch 3WE4, 3WE5 for actuating shaft 12x 12 mm Size 6, Handle black",114,"ST",null,"LP",0.32300000000000001,1,"8UC9385"]
["8US1921-2AB01","Busbar system, accessories Busbar center-to-center spacing 40, 60 mm Connection terminal Bar thickness: 5 mm 4-35 mm2",3.89,"ST",null,"LP",4.5999999999999999E-2,15,"8US19212AB01"]
["8US1998-1CA00","Busbar system, accessories Busbar center-to-center spacing 40, 60 mm Screw holder for SIRIUS Size S00, S0",124,"ST",100,"LP",3.0000000000000001E-3,20,"8US19981CA00"]
["8WA1821","Intermediate plate for terminals Sz. 6 and 16",0.68,"ST",null,"LP",3.0000000000000001E-3,50,"8WA1821"]
["8WA1871","Reduction plug","On Request","ST",null,"LP",5.0000000000000001E-3,10,"8WA1871"]
["8WA8360-0AF","inscription label, front, with 101-200, horizontal, terminal width: 5 mm, H: 7 mm, white",7.75,"ST",100,"LP",1E-4,204,"8WA83600AF"]
["8WA8361-0BS","inscription label, front, with 81-85, vertical, terminal width: 5 mm, H: 7 mm, white",7.75,"ST",100,"LP",1E-4,204,"8WA83610BS"]
["8WA8860-0BJ","inscription label, front, with 41-45, horizontal, terminal width: 5 mm, H: 7 mm, white","On Request","ST",1,"LP",1E-4,200,"8WA88600BJ"]
["8WH1000-1MG88","Fuse terminal LED 110-250 V with screw terminal Terminal size 4.0 mm2 Terminal width 6.2 mm Color black fuse 5x 20 mm",9.3000000000000007,"ST",null,"LP",1.7000000000000001E-2,50,"8WH10001MG88"]
["8WH1025-0AF00","Two-tier terminals with screw terminal Terminal size 2.5 mm2 Terminal width 5.2 mm Color gray with potential link",4.53,"ST",null,"LP",1.6E-2,50,"8WH10250AF00"]
["8WH2020-4CF00","Two-tier terminals with spring-loaded connection, top to bottom L, Cross-section: 0.08-2.5 mm2, Width: 5.2mm, Color: gray",2.3199999999999998,"ST",null,"LP",1.0999999999999999E-2,50,"8WH20204CF00"]
["8WH3000-0AE01","Through-type terminals with quick-connect technology Cross-section: 0.25-1.5 mm2, Width: 5.2mm, Color: blue",0.92,"ST",null,"LP",8.0000000000000002E-3,50,"8WH30000AE01"]
["8WH8120-4AB55","Labeling plate, front, with 51-60, vertical, Terminal width: 8.2 mm, H: 10.5 mm, white",5.69,"ST",100,"LP",2E-3,100,"8WH81204AB55"]
["8WH8121-2AB15","Labeling plate, flat, with 11-20, vertical, Terminal width: 5.2 mm, H: 6.4 mm, white",5.41,"ST",100,"LP",1E-4,100,"8WH81212AB15"]
["8WH8203-1AA05","Labeling plate, front, horizontal und vertical, Terminal width: 4.2 mm, H: 10.5 mm, white",5.32,"ST",100,"LP",1E-4,1200,"8WH82031AA05"]
["8WH9010-0BC08","ALPHA, Shorting plug",6.12,"ST",null,"LP",8.0000000000000002E-3,10,"8WH90100BC08"]
["8WH9040-1CB07","Plug-in coupling right element can be assembled by the user, with spring-loaded connection Cross-section: 0.08-2.5 mm2, Width: 5.2mm, Color: green-yellow",1.21,"ST",null,"LP",3.0000000000000001E-3,50,"8WH90401CB07"]
["8WH9066-5AA06","inscription label, with lightning symbol, vertical, terminal width: 16.2 mm, yellow",52.1,"ST",100,"LP",2E-3,25,"8WH90665AA06"]
["XPT:8PT1010","Door IP54 H2200 W400 right","On Request","ST",null,"LP",15.856,1,"XPT:8PT1010"]
["XPT:8PT9946","Cover 300 mm 165_5/100 8UC61","On Request","ST",null,"LP",3.34,5,"XPT:8PT9946"]
["3RA1345-8XB30-1AL2","Reversing contactor assembly AC-3, 37 kW/400 V,  3-pole Size S3, Screw terminal 230 V AC, 50/60 Hz Electrical and mechanical interlock !!! Phased-out product !!! Successor is SIRIUS 3RA2 Preferred successor type is >>3RA2338-8XB30-1AL2<<","On request","ST",1,"CP",4.3650000000000002,1,"3RA13458XB301AL2"]
["3RA1952-2E","Base plate for mounting of combination of three contactors (2x 3RT1.5, 1x 3RT2.4) for star-delta (wye-delta) start up",107,"ST",1,"CP",1.83,1,"3RA19522E"]
["3RA2110-0BD15-1FB4","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S00 0.14...0.20 A 24 V DC screw terminal for 60 mm busbar systems (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO (contactor) with diode (integrated)",114,"ST",1,"CP",1.1000000000000001,1,"3RA21100BD151FB4"]
["3RA2110-1DE15-1AP0","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S00 2.20...3.20 A 230 V AC Spring-type terminal for installation on standard mounting rail (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO (contactor)",91.1,"ST",1,"CP",0.69099999999999995,1,"3RA21101DE151AP0"]
["3RA2110-1GS15-1BB4","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S00 4.50...6.30 A 24 V DC Spring-type terminal for 60 mm busbar systems Type of coordination 1, Iq = 150 kA 1 NO (contactor) Adapter length 200 mm",122,"ST",1,"CP",1.1879999999999999,1,"3RA21101GS151BB4"]
["3RA2120-4AD26-0AP0","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S0 10...16 A 230 V AC screw terminal for 60 mm busbar systems (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO+1 NC (contactor)",163,"ST",1,"CP",1.282,1,"3RA21204AD260AP0"]
["3RA2125-1KE24-0FB4","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S0 9.00...12.5 A 24 V DC Spring-type terminal for installation on standard mounting rail (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO+1 NC (contactor) with diode combination plugged in at the front",173,"ST",1,"CP",1.2,1,"3RA21251KE240FB4"]
["3RA2210-0DE15-2BB4","Load feeder fuseless, Reversing duty 400 V AC, Size S00 0.22...0.32 A 24 V DC Spring-type terminal for installation on standard mounting rail (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NC (contactor)",128,"ST",1,"CP",1.0409999999999999,1,"3RA22100DE152BB4"]
["3RA2210-0KD15-2BB4","Load feeder fuseless, Reversing duty 400 V AC, Size S00 0.90...1.25 A 24 V DC screw terminal for 60 mm busbar systems (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NC (contactor)",179,"ST",1,"CP",1.77,1,"3RA22100KD152BB4"]
["3RA2220-1FB24-0AP0","Load feeder fuseless, Reversing duty 400 V AC, Size S0 3.50...5.00 A 230 V AC screw terminal for installation on standard mounting rail with standard mounting rail adapter (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO+1 NC (contactor)",182,"ST",1,"CP",1.5549999999999999,1,"3RA22201FB240AP0"]
["3RA2220-1KB24-0BB4","Load feeder fuseless, Reversing duty 400 V AC, Size S0 9.00...12.5 A 24 V DC screw terminal for installation on standard mounting rail with standard mounting rail adapter (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO+1 NC (contactor)",253,"ST",1,"CP",1.94,1,"3RA22201KB240BB4"]
["3RA2315-8XE30-1BB4","Reversing contactor assembly for 3RA27 AC-3, 3 kW/400 V, 24 V DC 3-pole, Size S00 screw terminal electrical and mechanical interlock with voltage tap",84.1,"ST",1,"CP",0.622,1,"3RA23158XE301BB4"]
["3RA2318-8XB30-2BB4","Reversing contactor assembly AC-3, 7.5 kW/400 V, 24 V DC 3-pole, Size S00 Spring-type terminal electrical and mechanical interlock",159,"ST",1,"CP",0.74,1,"3RA23188XB302BB4"]
["3RA2326-8XE30-1BB4","Reversing contactor assembly for 3RA27 AC-3, 11 kW/400 V, 24 V DC 3-pole, Size S0 screw terminal electrical and mechanical interlock 2 NO integrated, with voltage tap",242,"ST",1,"CP",1.327,1,"3RA23268XE301BB4"]
["3RA2423-8XE32-1BB4","cont. ass. f. star-delta (wye-delta) start, I/O-Link AC-3, 11 kW/400 V, 24 V DC 3-pole, size S0 screw terminals electrical and mechanical interlock 3 NO + 3 NC integrated",447,"ST",1,"CP",2.5110000000000001,1,"3RA24238XE321BB4"]
["3RA2712-1CA00","Function module for AS-i, star-delta (wye-delta) start screw terminal, Installation on contactors 3RT2 Communication-capable contactor required",187,"ST",1,"CP",0.23,1,"3RA27121CA00"]
["3RA2921-2GA00","Link module Electrical and mechanical for 3RV2021 and 3RW3.2, 3RW402 Spring-type terminal",16.700000000000003,"ST",1,"CP",0.09,1,"3RA29212GA00"]
["3RA2932-2F","Base plate, Size S2 for setting up contactor assemblies for star-delta (wye-delta) start comprising contactors in identical or different size",27.200000000000003,"ST",1,"CP",0.25700000000000001,1,"3RA29322F"]
["3RA6250-1DP32","SIRIUS Compact load feeder Reversing starter 690 V 110...240 V AC/DC 50...60 Hz 3...12 A IP20 Connection main circuit: Screw terminal Connection control circuit: screw terminal",640,"ST",1,"CP",2.569,1,"3RA62501DP32"]
["3RA6500-1BB43","SIRIUS Compact load feeder Reversing starter for IO-Link 690 V 24 V DC 0.32...1.25 A IP20 Connection main circuit: plug-in, without terminals Connection control circuit: screw terminal",655,"ST",1,"CP",2.4700000000000002,1,"3RA65001BB43"]
["3RB2133-4QD0","Overload relay 6...25 A For motor protection Size S2, Class 5...30 Contactor mounting Main circuit: Screw terminal Auxiliary circuit: Spring-type terminal Manual-Automatic-Reset Internal ground fault detection !!! Phased-out product !!! Successor is SIRIUS 3RB3 Preferred successor type is >>3RB3123-4QE0<<","On request","ST",1,"CP",0.35,1,"3RB21334QD0"]
["3RB3016-1PE0","Overload relay 1...4 A Electronic For motor protection Size S00, Class 10E Contactor mounting Main circuit: Spring-type terminal Auxiliary circuit: Spring-type terminal Manual-Automatic-Reset",56.9,"ST",1,"CP",0.22500000000000001,1,"3RB30161PE0"]
["3RF2030-1AA04","Semiconductor relay, 1-phase 3RF2 Overall width 45 mm, 30 A 48-460 V / 24 V DC screw terminal",42.800000000000004,"ST",1,"CP",8.4000000000000005E-2,1,"3RF20301AA04"]
["3RF2090-1AA45","Semiconductor relay, 1-phase 3RF2 Overall width 45 mm, 90 A 48-600 V / 4-30 V DC screw terminal Blocking voltage 1200 V",72.599999999999994,"ST",1,"CP",8.5000000000000006E-2,1,"3RF20901AA45"]
["3RF2310-3AA26","Solid-state contactor 1-phase 3RF2 AC 51 / 10 A / 40 Β°C 48-600 V / 110-230 V AC Ring cable connection",81.599999999999994,"ST",1,"CP",0.16600000000000001,1,"3RF23103AA26"]
["3RF2320-2AA24","Solid-state contactor 1-phase 3RF2 AC 51 / 20 A / 40 Β°C 48-460 V / 110-230 V AC Spring-type terminal",71.899999999999991,"ST",1,"CP",0.23300000000000001,1,"3RF23202AA24"]
["3RF2410-1AB55","Solid-state contactor 3-phase 3RF2 AC 51 / 10 A / 40 Β°C 48-600 V / 230 V AC 2-phase controlled screw terminal Blocking voltage 1200 V",142,"ST",1,"CP",0.35499999999999998,1,"3RF24101AB55"]
["3RF2916-0JA16-1KK0","Heat current monitoring Current range 16 A / 40 Β°C 400-600 V / 24 V AC/DC for semiconductor relay / contactor Remote teach/without control connector Customer-specific version",138,"ST",1,"CP",0.17100000000000001,1,"3RF29160JA161KK0"]
["3RG9220-0AA00","AS-Interface coupling module PG with 4 entries PG11 for standard round cable",38.9,"ST",1,"CP",0.105,1,"3RG92200AA00"]
["3RH1921-2FA04","Auxiliary switch block, 4 NC, EN 50005 Spring type, size S0 ... S12 for contactor relays and motor contactors ! Phased-out product! Successor is SIRIUS 3RH2","On request","ST",1,"CP",6.9000000000000006E-2,1,"3RH19212FA04"]
["3RH2122-2KB40","Coupling contactor relay, 2 NO + 2 NC, 24 V DC, 0.7 ... 1.25* US, with integrated suppressor diode, Size S00, Spring-type terminal suitable for PLC outputs",38.300000000000004,"ST",1,"CP",0.316,1,"3RH21222KB40"]
["3RH2122-4AG60","Contactor relay, 2 NO + 2 NC, 100 V AC, 50 Hz, 100 .. 110 V, 60 Hz, Size S00, ring cable lug connection",32.5,"ST",1,"CP",0.22800000000000001,1,"3RH21224AG60"]
["3RH2131-2AH00","Contactor relay, 3 NO + 1 NC, 48 V AC, 50 / 60 Hz, Size S00, Spring-type terminal",29.400000000000002,"ST",1,"CP",0.255,1,"3RH21312AH00"]
["3RH2140-2JC40","Coupling contactor relay, 4 NO, 30 V DC, 0.7 ... 1.25* US, with integrated diode, Size S00, Spring-type terminal suitable for PLC outputs",38.800000000000004,"ST",1,"CP",0.318,1,"3RH21402JC40"]
["3RH2271-1AP60","Contactor relay, 7 NO + 1 NC, 220 V AC, 50 Hz / 240 V, 60 Hz, Size S00, screw terminal, Captive auxiliary switch, for SUVA applications",49,"ST",1,"CP",0.29299999999999998,1,"3RH22711AP60"]
["3RH2911-1DA20","Auxiliary switch lateral, 2 NO Current path 1 NO, 1 NO for 3RH and 3RT screw terminal R: 23/24, 33/34 L: 43/44, 53/54",13.299999999999999,"ST",1,"CP",0.04,1,"3RH29111DA20"]
["3RH2911-1NF11","Electron. contr. auxiliary switch 1 NO+1 NC, Current path 1 NO,--,--, 1 NC front-side for 3RH and 3RT screw terminal .3/.4, --/--, --/--, .1/.2",33.800000000000004,"ST",1,"CP",4.2000000000000003E-2,1,"3RH29111NF11"]
["3RK1200-0CE02-0AA2","AS-i SlimLine module Phased-out product !!! For further information, please contact our sales department S22.5 digital 4 DI, IP20 4 x inputs for 3-wire sensor Screw terminals Overall width 22.5 mm",222,"ST",1,"CP",0.13800000000000001,1,"3RK12000CE020AA2"]
["3RK1301-0CB10-1AB4","RS1E-X for ET200S High Feature reversing starter Setting range 2.4...16 A Mechanical switching Electronic protection AC-3, up to 7.5 kW / 400 V expandable for Brake control module 2DI module 2DI module Motor starter ES Circuit breaker signaling parameterizable DPV 1-capable PROFIENERGY-capable to PN",788,"ST",1,"CP",2.3839999999999999,1,"3RK13010CB101AB4"]
["3RK1325-6KS41-0AA0","SIRIUS motor starter M200D AS-i Communication: AS-Interface DOL starter Standard Mechanical switching AC-3, 0.75KW / 400 V 0.15 A...2.00 A Electronic overload protection Electronic overload protection Thermistor: THERMOCLICK / PTC without brake contact 4 DI/1 DO AS-i Han Q4/2 - Han Q8/0",863,"ST",1,"CP",3.7440000000000002,1,"3RK13256KS410AA0"]
["3RK1325-6LS41-3AA0","SIRIUS motor starter M200D AS-i Communication: AS-Interface Reversing starter standard Mechanical switching AC-3, 5.5 kW / 400 V 1.5 A...12.00 A Electronic overload protection Thermistor: THERMOCLICK / PTC without brake contact 4 DI / 1 DO AS-i Han Q4/2 - Han Q8/0 with manual on-site operation and key-operated switch",1085,"ST",1,"CP",3.984,1,"3RK13256LS413AA0"]
["3RK1405-1SE15-0AA2","ASIsafe SlimLine module S45F digital safety IP20 1F-RQ/3DI/2DQ 1 x safe output Relay 2-channel 3 x standard input 2 x standard output 24 V DC Screw terminals Overall width 45 mm",505,"ST",1,"CP",0.35,1,"3RK14051SE150AA2"]
["3RK1901-1NR04","AS-Interface 4-fold M12 feeder U_ASI and Uaux, 4 x M12 socket IP67 Delivery incl. mounting plate",104,"ST",1,"CP",0.11,1,"3RK19011NR04"]
["3RK1908-0AP00-0CP0","Base unit for ET 200SP motor starter with infeed 500 V including cover infeed bus",161,"ST",1,"CP",0.17,1,"3RK19080AP000CP0"]
["3RK1911-2AG00","Data T piece (copper) for PROFIBUS DP (hybrid)","On request","ST",1,"CP",0.1,1,"3RK19112AG00"]
["3RK4320-3GR51-0BA0","SIRIUS MCU motor starter Enclosure degree of protection IP55 plastic Communication AS-Interface electromechanically switching Short-circuit protection with circuit breaker DOL starter Brake without Performance class 2.50 A Motor circuit breaker with bi-metal thermal Manual operation without Connection power M screw connection Standard product",878,"ST",1,"CP",2.14,1,"3RK43203GR510BA0"]
["3RK4324-3ER51-1BC0","SIRIUS MCU motor starter Enclosure degree of protection IP54 plastic Communication AS-Interface electromechanically switching Short-circuit protection with circuit breaker Reversing starter Brake without Performance class 1.6 A Motor circuit breaker with bi-metal thermal without manual operation Connection power M screw connection Special variant new design A/B slave AS-i SPEC V2.1 Sensor-actuator 1x AS-i 3xDI/DO Supply sensor U-AUX",1184,"ST",1,"CP",1.744,1,"3RK43243ER511BC0"]
["3RK4340-3JR51-0BA0","SIRIUS MCU motor starter Enclosure degree of protection IP55 plastic Communication without electromechanically switching Short-circuit protection with circuit breaker DOL starter Brake without Performance class 4.00 A Motor circuit breaker with bi-metal thermal Manual operation without Connection power M screw connection Standard product",550,"ST",1,"CP",1.98,1,"3RK43403JR510BA0"]
["3RM1910-1AA","Accessory for SIRIUS 3RM1 3-phase busbar for 2 motor starters Modular spacing 22.5 mm Screw connection system",7.6,"ST",1,"CP",1.9E-2,1,"3RM19101AA"]
["3RP1505-2RW30","Timing relay, Multifunction Phased-out product !!! For further information, please contact our sales department Spring-type terminal 2 change-over contacts, 8 functions Positively driven 24...240 V AC/DC at 50/60 Hz AC 15 time ranges (0.05 s-100 h)",248,"ST",1,"CP",0.14799999999999999,1,"3RP15052RW30"]
["3RP1540-1BN31","Timing relay, electronic Phased-out product !!! For further information, please contact our sales department OFF delay 2 change-over contacts, without auxiliary voltage 9 time ranges, 0.05 s...600 s 200...240 V AC/DC with LED, Screw terminal",199,"ST",1,"CP",0.156,1,"3RP15401BN31"]
["3RP1578-1NQ38-0AB2","Timing relay, star-delta (wye-delta) Phased-out product !!! For further information, please contact our sales department 1 NO delayed, 1 NO instantaneous 20 s runtime, 120 ms pause 24 V AC/DC and 100-127 V AC at 50/60 Hz AC",113,"ST",1,"CP",0.115,1,"3RP15781NQ380AB2"]
["3RQ3055-2SM30","Output coupler Optocoupler 1 NO, Transistor, 24 V DC Output max. 30 V DC, 5 A short circuit-proof Spring-type terminal (push-in) Overall width 6.2 mm Thermal current 5A",53.1,"ST",1,"CP",3.1E-2,5,"3RQ30552SM30"]
["3RS1101-1CK20","Temperature monitoring relay Thermocouple type K, overshoot 1 threshold value, Width 22.5 mm 0 Β°C to 200 Β°C 110-120/220-240 V AC 1 NO + 1 NC, quiescent current principle screw terminal",143,"ST",1,"CP",0.17299999999999999,1,"3RS11011CK20"]
["3RS1703-1AE00","interface converter Phased-out product !!! For further information, please contact our sales department 24 V AC/DC, 3-way separation input: 4-20 mA output: 0-10 V screw terminal","On request","ST",1,"CP",7.0999999999999994E-2,1,"3RS17031AE00"]
["3RS1800-2HP01","!!! Phased-out product !!! The preferred successor is 3RQ2000-2CW01. Coupling relays in industrial enclosure 3 change-over contacts hard gold-plated Combination voltage 24 V and 220-240 V AC/DC Spring-type terminal",68.699999999999989,"ST",1,"CP",0.14599999999999999,1,"3RS18002HP01"]
["3RT1034-1AN24","Power contactor, AC-3 32 A, 15 kW / 400 V 220 V AC, 50 / 60 Hz, 2 NO + 2 NC, 3-pole, Size S2, Screw terminal !!! Phased-out product !!! Successor is SIRIUS 3RT2 Preferred successor type is >>3RT2027-1AN24<<","On request","ST",1,"CP",0.90800000000000003,1,"3RT10341AN24"]
["3RT1034-1BE44","Power contactor, AC-3 32 A, 15 kW / 400 V 60 V DC, 2 NO + 2 NC, 3-pole, Size S2 Screw terminal !!! Phased-out product !!! Successor is SIRIUS 3RT2","On request","ST",1,"CP",1.5369999999999999,1,"3RT10341BE44"]
["3RT1035-1AD20","Power contactor, AC-3 40 A, 18.5 kW / 400 V 42 V AC, 50 / 60 Hz, 3-pole, Size S2, Screw terminal !!! Phased-out product !!! Successor is SIRIUS 3RT2","On request","ST",1,"CP",0.83299999999999996,1,"3RT10351AD20"]
["3RT1035-1BW40","Power contactor, AC-3 40 A, 18.5 kW / 400 V 48 V DC, 3-pole, Size S2, Screw terminal !!! Phased-out product !!! Successor is SIRIUS 3RT2 Preferred successor type is >>3RT2028-1BW40<<","On request","ST",1,"CP",1.4219999999999999,1,"3RT10351BW40"]
["3RT1035-3XP00-0GA0","Power contactor, AC-3 40 A, 18.5 kW / 400 V 230 V AC, 50 / 60 Hz, 3-pole, Size S2 Spring-type terminal With electronic control unit With varistor attenuated low-noise !!! Phased-out product !!! Successor is SIRIUS 3RT2 Preferred successor type is >>3RT2035-3NP30<<","On request","ST",1,"CP",1.4430000000000001,1,"3RT10353XP000GA0"]
["3RT1036-3AD20","Power contactor, AC-3 50 A, 22 kW / 400 V 42 V AC, 50 / 60 Hz, 3-pole, Size S2, Spring-type terminal !!! Phased-out product !!! Successor is SIRIUS 3RT2","On request","ST",1,"CP",0.84699999999999998,1,"3RT10363AD20"]
["3RT1044-1BD44","Power contactor, AC-3 65 A, 30 kW / 400 V 42 V DC, 2 NO + 2 NC, 3-pole, Size S3, Screw terminal !!! Phased-out product !!! Successor is SIRIUS 3RT2","On request","ST",1,"CP",2.8740000000000001,1,"3RT10441BD44"]
["3RT1044-3BW40","Power contactor, AC-3 65 A, 30 kW / 400 V 48 V DC, 3-pole, Size S3 Spring-type terminal !!! Phased-out product !!! Successor is SIRIUS 3RT2","On request","ST",1,"CP",2.8069999999999999,1,"3RT10443BW40"]
["3RT1045-3AF00","Power contactor, AC-3 80 A, 37 kW / 400 V 110 V AC, 50 Hz 3-pole, Size S3 Spring-type terminal !!! Phased-out product !!! Successor is SIRIUS 3RT2 Preferred successor type is >>3RT2038-3AF00<<","On request","ST",1,"CP",1.8480000000000001,1,"3RT10453AF00"]
["3RT1046-1AB04","Power contactor, AC-3 95 A, 45 kW / 400 V 24 V AC, 50 Hz, 2 NO + 2 NC 3-pole, Size S3 Screw terminal !!! Phased-out product !!! Successor is SIRIUS 3RT2 Preferred successor type is >>3RT2046-1AB04<<","On request","ST",1,"CP",1.9410000000000001,1,"3RT10461AB04"]
["3RT1046-1AV60","Power contactor, AC-3 95 A, 45 kW / 400 V 480 V AC, 60 Hz 3-pole, Size S3 Screw terminal !!! Phased-out product !!! Successor is SIRIUS 3RT2 Preferred successor type is >>3RT2046-1AV60<<","On request","ST",1,"CP",1.8460000000000001,1,"3RT10461AV60"]
["3RT1054-3AD36","Power contactor, AC-3 115 A, 55 kW / 400 V AC (50-60 Hz) / DC operation 42-48 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, Size S6 with box terminals Drive: conventional Spring-type terminal",364,"ST",1,"CP",3.6160000000000001,1,"3RT10543AD36"]
["3RT1055-2NF36","Power contactor, AC-3 150 A, 75 kW / 400 V AC (50-60 Hz) / DC operation 96-127 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, Size S6 Busbar connections Drive: electronic with PLC interface 24 V DC Spring-type terminal",464,"ST",1,"CP",3.3330000000000002,1,"3RT10552NF36"]
["3RT1064-2AM36","Power contactor, AC-3 225 A, 110 kW / 400 V AC (50-60 Hz) / DC operation 200-220 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, Size S10 Busbar connections Drive: conventional Spring-type terminal",705,"ST",1,"CP",6.4909999999999997,1,"3RT10642AM36"]
["3RT1065-6AD36","Power contactor, AC-3 265 A, 132 kW / 400 V AC (50-60 Hz) / DC operation 42-48 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, Size S10 Busbar connections Drive: conventional screw terminal",880,"ST",1,"CP",6.5659999999999998,1,"3RT10656AD36"]
["3RT1076-6AV36","Power contactor, AC-3 500 A, 250 kW / 400 V AC (50-60 Hz) / DC 380-420 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, size S12 Busbar connections Operating mechanism: conventional screw terminals",1521,"ST",1,"CP",10.394,1,"3RT10766AV36"]
["3RT1265-6AP36","Vacuum contactor, AC-3 265 A, 132 kW / 400 V AC (50-60 Hz) / DC operation 220-240 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, Size S10 Busbar connections Drive: conventional",1409,"ST",1,"CP",7.3,1,"3RT12656AP36"]
["3RT1346-1AK60","Contactor, AC-1, 140 A, 120 V AC, 60 Hz, 4-pole, Size S3, Screw terminal !!! Phased-out product !!! Successor is SIRIUS 3RT2","On request","ST",1,"CP",2.1739999999999999,1,"3RT13461AK60"]
["3RT1466-6PP35","Contactor, AC-1, 400 A 230 (50...60 Hz) / DC operation 200 ... 277 V UC Auxiliary contacts 1 NO + 1 NC 3-pole, Size S10 Busbar connections Drive: electronic with PLC / SIMOCODE interface and RLT signal",1174,"ST",1,"CP",7,1,"3RT14666PP35"]
["3RT1647-1AV01","Capacitor contactor, AC-6, 50 kVAr / 400 V, 400 V, 50 Hz, 3-pole, Size S3 !!! Phased-out product !!! Successor is SIRIUS 3RT2","On request","ST",1,"CP",1.875,1,"3RT16471AV01"]
["3RT1926-3AF31","Latching block, mechanical, for mounting on 3RT1.2. and 3RT1.3., 110 V AC/DC, ! Phased-out product! Successor is SIRIUS 3RT2","On request","ST",1,"CP",0.128,1,"3RT19263AF31"]
["3RT1935-6A","Replacement contact pieces for contactor Size S2, 3-pole, AC-3, 18.5 kW, 3 NO, main contacts, Consists of 3 movable and 6 fixed contacts with mounting parts !!! Phased-out product !!! Successor is SIRIUS 3RT2","On request","ST",1,"CP",4.3999999999999997E-2,1,"3RT19356A"]
["3RT1944-5AG22","Magnet coil for contactors SIRIUS, Size S3, spring-loaded connection technology 110 V AC, 50 / 60 Hz !!! Phased-out product !!! Successor is SIRIUS 3RT2","On request","ST",1,"CP",0.17599999999999999,1,"3RT19445AG22"]
["3RT1945-5AN61","Magnet coil for contactors SIRIUS, Size S3 Screw terminal 200 V AC, 50 / 60 Hz, 220 V, 60 Hz !!! Phased-out product !!! Successor is SIRIUS 3RT2","On request","ST",1,"CP",0.17100000000000001,1,"3RT19455AN61"]
["3RT1956-4G","Box terminal for contactor 3RT1, 3RB2 Size S6 max. connection approx. 120 mm2",38.9,"ST",1,"CP",0.26200000000000001,1,"3RT19564G"]
["3RT1966-4PA00","Connection part set M 10 x 30 complete for one contactor",8.2999999999999989,"ST",1,"CP",0.25600000000000001,1,"3RT19664PA00"]
["3RT2015-1BB42","Power contactor, AC-3 7 A, 3 kW / 400 V 1 NC, 24 V DC 3-pole, Size S00 screw terminal",30.200000000000003,"ST",1,"CP",0.29099999999999998,1,"3RT20151BB42"]
["3RT2015-1QB42","Power contactor, AC-3 7 A, 3 kW / 400 V 1 NC, 24 V DC 0.7-1.25* US, with varistor plugged on, 3-pole, Size S00, screw terminal",34.9,"ST",1,"CP",0.312,1,"3RT20151QB42"]
["3RT2016-1AU02","Power contactor, AC-3 9 A, 4 kW / 400 V 1 NC, 240 V AC, 50 / 60 Hz 3-pole, Size S00 screw terminal",26.900000000000002,"ST",1,"CP",0.23599999999999999,1,"3RT20161AU02"]
["3RT2016-2AP02","Power contactor, AC-3 9 A, 4 kW / 400 V 1 NC, 230 V AC, 50 / 60 Hz 3-pole, Size S00 Spring-type terminal",26.900000000000002,"ST",1,"CP",0.25,1,"3RT20162AP02"]
["3RT2016-2XF42-0LA2","Traction contactor, AC-3 9 A, 4 kW / 400 V 1 NC, 72 - 125 V DC, 0.7-1.25* US with integrated varistor Size S00, Spring-type terminal suitable for PLC outputs",57.6,"ST",1,"CP",0.32600000000000001,1,"3RT20162XF420LA2"]
["3RT2017-1BA41","Power contactor, AC-3 12 A, 5.5 kW / 400 V 1 NO, 12 V DC 3-pole, Size S00 screw terminal",39.800000000000004,"ST",1,"CP",0.29499999999999998,1,"3RT20171BA41"]
["3RT2017-2KF42","power contactor, AC-3 12 A, 5.5 kW / 400 V 1 NC, 110 V DC 0.7-1.25*US with integrated suppressor diode 3-pole, Size S00 Spring-type terminal suitable for PLC outputs",40.6,"ST",1,"CP",0.316,1,"3RT20172KF42"]
["3RT2018-1AD01","Power contactor, AC-3 16 A, 7.5 kW / 400 V 1 NO, 42 V AC, 50/60 Hz 3-pole, Size S00 screw terminals",44,"ST",1,"CP",0.23300000000000001,1,"3RT20181AD01"]
["3RT2018-1UB42","Contactor, AC-3, 7.5 kW / 400 V, 1 NC, 24 V DC with varistor integrated, 3-pole, Screw terminal",74.099999999999994,"ST",1,"CP",0.28999999999999998,1,"3RT20181UB42"]
["3RT2023-1AF00","power contactor, AC-3 9 A, 4 kW / 400 V 1 NO + 1 NC, 110 V AC, 50 Hz 3-pole, Size S0 screw terminal",30,"ST",1,"CP",0.40600000000000003,1,"3RT20231AF00"]
["3RT2024-1BM44","power contactor, AC-3 12 A, 5.5 kW / 400 V 2 NO + 2 NC, 220 V DC 3-pole, Size S0 screw terminal Removable auxiliary switch",76.099999999999994,"ST",1,"CP",0.6,1,"3RT20241BM44"]
["3RT2024-2AP00","power contactor, AC-3 12 A, 5.5 kW / 400 V 1 NO + 1 NC, 230 V AC, 50 Hz 3-pole, Size S0 Spring-type terminal",33.4,"ST",1,"CP",0.443,1,"3RT20242AP00"]
["3RT2025-1AK60-1AA0","power contactor, AC-3 17 A, 7.5 kW / 400 V 1 NO + 1 NC, 110 V AC, 50 Hz, 120 V, 60 Hz, 3-pole, Size S0, screw terminal upright mounting position",50.4,"ST",1,"CP",0.42,1,"3RT20251AK601AA0"]
["3RT2026-1AH00","power contactor, AC-3 25 A, 11 kW / 400 V 1 NO + 1 NC, 48 V AC, 50 Hz, 3-pole, Size S0 screw terminal",62.4,"ST",1,"CP",0.41599999999999998,1,"3RT20261AH00"]
["3RT2026-2CL24-3MA0","power contactor, AC-3 25 A, 11 kW / 400 V 2 NO + 2 NC, 230 V AC 50 / 60 Hz, with inserted varistor, 3-pole, Size S0 Spring-type terminal Captive auxiliary switch for SUVA applications",84.199999999999989,"ST",1,"CP",0.51800000000000002,1,"3RT20262CL243MA0"]
["3RT2027-1AN60","Power contactor, AC-3 32 A, 15 kW / 400 V 1 NO + 1 NC, 200 V AC, 50 Hz 200-220 V, 60Hz, 3-pole Size S0, screw terminals",89.399999999999991,"ST",1,"CP",0.42399999999999999,1,"3RT20271AN60"]
["3RT2027-1FB40","Power contactor, AC-3 32 A, 15 kW / 400 V 1 NO + 1 NC, 24 V DC with plugged-in diode combination, 3-pole Size S0, screw terminals",147,"ST",1,"CP",0.60799999999999998,1,"3RT20271FB40"]
["3RT2028-1BB40-1AA0","Power contactor, AC-3 38 A, 18.5 kW / 400 V 1 NO + 1 NC, 24 V DC 3-pole, size S0 screw terminals Upright mounting position",148,"ST",1,"CP",0.60199999999999998,1,"3RT20281BB401AA0"]
["3RT2028-2BM40","Power contactor, AC-3 38 A, 18.5 kW / 400 V 1 NO + 1 NC, 220 V DC 3-pole, size S0 Spring-type terminals",141,"ST",1,"CP",0.64200000000000002,1,"3RT20282BM40"]
["3RT2035-3NF30","power contactor, AC-3 40 A, 18.5 kW / 400 V 1 NO + 1 NC, AC / DC 84-155 V, with varistor, 3-pole, Size S2, Spring-type terminal",165,"ST",1,"CP",1.1120000000000001,1,"3RT20353NF30"]
["3RT2036-1AV04","power contactor, AC-3 50 A, 22 kW / 400 V 2 NO + 2 NC, 400 V AC, 50 Hz, 3-pole, Size S2, screw terminal",147,"ST",1,"CP",1.0649999999999999,1,"3RT20361AV04"]
["3RT2037-1NF30","Power contactor, AC-3 65 A, 30 kW / 400 V 1 NO + 1 NC, 84-155 V AC / DC with varistor 3-pole, size S2 screw terminals",275,"ST",1,"CP",1.129,1,"3RT20371NF30"]
["3RT2037-3XF40-0LA2","Traction contactor, AC-3 65 A, 30 kW / 400 V 1 NO + 1 NC 110 V DC, 0.7-1.25* Us with varistor 3-pole, size S2 Spring-type terminals",383,"ST",1,"CP",1.117,1,"3RT20373XF400LA2"]
["3RT2045-1CP04-3MA0","power contactor, AC-3 80 A, 37 kW / 400 V 2 NO + 2 NC, 230 V AC/50 Hz 3-pole, 3 NO, Size S3 screw terminal Inserted varistor Captive auxiliary switch",243,"ST",1,"CP",1.772,1,"3RT20451CP043MA0"]
["3RT2046-1AL00","power contactor, AC-3 95 A, 45 kW / 400 V 1 NO + 1 NC, 125 V AC, 50 Hz 3-pole, 3 NO, Size S3 screw terminal",282,"ST",1,"CP",1.7190000000000001,1,"3RT20461AL00"]
["3RT2047-1AP00-1AA0","Power contactor, AC-3 115 A, 55 kW /  400 V 1 NO + 1 NC, 230 V AC, 50 Hz 3-pole, 3 NO, Size S3 screw terminals Upright mounting position",346,"ST",1,"CP",1.722,1,"3RT20471AP001AA0"]
["3RT2317-1AH00","Contactor, 4 NO, AC-1: 22 A 48 V AC, 50 / 60 Hz, 4-pole, 4 NO, Size S00, Screw terminal",32.200000000000003,"ST",1,"CP",0.23300000000000001,1,"3RT23171AH00"]
["3RT2327-2BB40","Contactor, 4 NO, AC-1: 50 A 24 V DC, 4-pole, 4 NO, size: S0, Spring-type terminal 1 NO + 1 NC integrated",145,"ST",1,"CP",0.77,1,"3RT23272BB40"]
["3RT2346-1AF00","Contactor, 4 NO, AC-1: 140 A 110 V AC/50 Hz 4-pole, 4 NO, Size S3 Screw terminal 1 NO+1 NC integrated",335,"ST",1,"CP",2.0550000000000002,1,"3RT23461AF00"]
["3RT2448-1NP30","Contactor, AC-1: 160 A 175-280 V AC/DC 3-pole, 3 NO, Size S3 Screw terminal 1 NO + 1 NC varistor integrated",354,"ST",1,"CP",1.8080000000000001,1,"3RT24481NP30"]
["3RT2526-2BF40","Power contactor, AC-3 25 A, 11 kW / 400 V 2 NO + 2 NC 110 V DC, 50 Hz 4-pole size S0 Spring-type terminals 1 NO + 1 NC integrated",126,"ST",1,"CP",0.71799999999999997,1,"3RT25262BF40"]
["3RT2617-1BB43","Capacitor contactor, AC-6b 12.5 kVAr, / 400 V 1 NO + 1 NC, 24 V DC 3-pole, Size S00 screw terminal",112,"ST",1,"CP",0.43,1,"3RT26171BB43"]
["3RT2916-1BD00","Surge suppressor, varistor, 127 ... 240 V AC 150 ... 250 V DC for contactor relays and motor contactors Size S00",8.1999999999999993,"ST",1,"CP",7.0000000000000001E-3,1,"3RT29161BD00"]
["3RT2924-5AT61","Magnet coil for contactors 7.5 kW 600 V AC, 60Hz, for motor contactors, Size S0, Screw terminal",22.5,"ST",1,"CP",7.4999999999999997E-2,1,"3RT29245AT61"]
["3RT2936-1BF00","Surge suppressor, varistor, 400 ... 600 V AC, for contactors Size S2, S3",15.299999999999999,"ST",1,"CP",7.0000000000000001E-3,1,"3RT29361BF00"]
["3RT2944-5NB31","Magnet coil for contactor S3, 20 ... 33 V AC/DC, with varistor",52.5,"ST",1,"CP",0.33,1,"3RT29445NB31"]
["3RU2116-1BB0","Overload relay 1.4...2.0 A Thermal For motor protection Size S00, Class 10 Contactor mounting Main circuit: Screw Auxiliary circuit: Screw Manual-Automatic-Reset",38.300000000000004,"ST",1,"CP",0.16500000000000001,1,"3RU21161BB0"]
["3RU2116-1HC1","Overload relay 5.5...8.0 A Thermal For motor protection Size S00, Class 10 Stand-alone installation Main circuit: Spring-type terminal Auxiliary circuit: spring-type terminal Manual-Automatic-Reset",49,"ST",1,"CP",0.21099999999999999,1,"3RU21161HC1"]
["3RU2136-4KB0","Overload relay 62...73 A Thermal For motor protection Size S2, Class 10A Contactor mounting Main circuit: Screw Auxiliary circuit: Screw Manual-Automatic-Reset",101,"ST",1,"CP",0.32600000000000001,1,"3RU21364KB0"]
["3RU2146-4MD1","Overload relay 80...100 A Thermal For motor protection Size S3, Class 10 Stand-alone installation Main circuit: Screw Auxiliary circuit: spring-type terminal Manual-Automatic-Reset",174,"ST",1,"CP",0.81499999999999995,1,"3RU21464MD1"]
["3RV1042-4JA10","Circuit breaker size S3 A-release 45...63 A Short-circuit release 819 A Motor protection up to 100 kA,Class 10 Screw terminal Increased switching capacity !!! Phased-out product !!! Successor is SIRIUS 3RV2 Preferred successor type is >>3RV2032-4JA10<<","On request","ST",1,"CP",2.2549999999999999,1,"3RV10424JA10"]
["3RV1341-4MC10","Circuit breaker size S3 For starter combination Rated current 100 A Short-circuit release 1235 A Screw terminal Standard switching capacity !!! Phased-out product !!! Successor is SIRIUS 3RV2 Preferred successor type is >>3RV2341-4MC10<<","On request","ST",1,"CP",2.2730000000000001,1,"3RV13414MC10"]
["3RV1913-4C","Molded plastic front plate Degree of protection IP55 with actuator diaphragm and holder for circuit breaker Size S00",23.3,"ST",1,"CP",0.20399999999999999,1,"3RV19134C"]
["3RV1923-1DA00","Molded-plastic enclosure for surface mounting Degree of protection IP55 with N and PE terminal Can be locked in O position 72 mm with metric cable gland No UL/CSA approval",17.700000000000003,"ST",1,"CP",0.36,1,"3RV19231DA00"]
["3RV1982-1ED0","Shunt release 110...127 V AC, 110...125 V DC for size 3RV1. 6, 7, 8",76.899999999999991,"ST",1,"CP",0.13700000000000001,1,"3RV19821ED0"]
["3RV2011-1HA25","Circuit breaker size S00 for motor protection, CLASS 10 A-release 5.5...8 A N-release 104 A Spring-type terminal Standard switching capacity with transverse auxiliary switches 1 NO+1 NC",66.699999999999989,"ST",1,"CP",0.38800000000000001,1,"3RV20111HA25"]
["3RV2021-1AA20-0BA0","Special type Circuit breaker size S0 for motor protection, CLASS 10 A-release 1.1...1.6 A N-release 21 A Spring-type terminal Standard switching capacity Ambient temperature -50 Β°C 500 switching cycles",79,"ST",1,"CP",0.4,1,"3RV20211AA200BA0"]
["3RV2031-4EA15","Circuit breaker size S2 for motor protection, CLASS 10 A-release 22...32 A N-release 416 A screw terminal Standard switching capacity with transverse auxiliary switches 1 NO+1 NC",160,"ST",1,"CP",1.0649999999999999,1,"3RV20314EA15"]
["3RV2111-1BA10","Circuit breaker size S00 for motor protection, CLASS 10 with overload relay function A-release 1.4...2 A N-release 26 A screw terminal Standard switching capacity",79.199999999999989,"ST",1,"CP",0.40699999999999997,1,"3RV21111BA10"]
["3RV2311-0KC20","Circuit breaker size S00 for starter combination Rated current 1.25 A N-release 16 A Spring-type terminal Standard switching capacity",43.5,"ST",1,"CP",0.36,1,"3RV23110KC20"]
["3RV2411-0AA20","Circuit breaker size S00 for transformer protection A-release 0.11...0.16 A N-release 3.3 A Spring-type terminal Standard switching capacity",55,"ST",1,"CP",0.29699999999999999,1,"3RV24110AA20"]
["3RV2411-1FA10","Circuit breaker size S00 for transformer protection A-release 3.5...5 A N-release 104 A screw terminal Standard switching capacity",56.6,"ST",1,"CP",0.34899999999999998,1,"3RV24111FA10"]
["3RV2431-4BA10","Circuit breaker size S2 for transformer protection A-release 14...20 A N-release 400 A screw terminal Standard switching capacity",99,"ST",1,"CP",1.0629999999999999,1,"3RV24314BA10"]
["3RV2915-5B","3-phase supply terminal for 3-phase busbar Size S0 and S00 connection from below",16.2,"ST",1,"CP",0.109,1,"3RV29155B"]
["3RV2946-2BB00-0AA4","Door-coupling rotary operating mechanism for circuit breaker Size S3 8UC7 handle black Display plate black Special inscription HAUNI",84.8,"ST",1,"CP",1.6459999999999999,1,"3RV29462BB000AA4"]
["3RW4026-2TB05","SIRIUS soft starter S0 25 A, 15 kW/500 V, 40 Β°C 400-600 V AC, 24 V AC/DC spring-type terminals Thermistor motor protection",619,"ST",1,"CP",0.76500000000000001,1,"3RW40262TB05"]
["3RW4046-1BB05","SIRIUS soft starter S3 80 A, 55 kW/500 V, 40 Β°C 400-600 V AC, 24 V AC/DC Screw terminals",1401,"ST",1,"CP",1.8759999999999999,1,"3RW40461BB05"]
["3RW4427-1BC34","SIRIUS soft starter Values at 460 V, 50 Β°C Standard: 82 A, 60 hp Inside-delta: 142 A, 100 hp 200-460 V AC, 115 V AC Screw terminals",2090,"ST",1,"CP",12.457000000000001,1,"3RW44271BC34"]
["3RW4435-6BC36","SIRIUS soft starter Values at 575 V, 50 Β°C Standard: 117 A, 100 hp Inside-delta: 203 A, 200 hp 400-690 V AC, 115 V AC Screw terminals",3525,"ST",1,"CP",8.1379999999999999,1,"3RW44356BC36"]
["3RW4455-6BC35","SIRIUS soft starter Values at 575 V, 50 Β°C Standard: 615 A, 700 hp Inside-delta: 1065 A, 1200 hp 400-600 V AC, 115 V AC Screw terminals",12483,"ST",1,"CP",62,1,"3RW44556BC35"]
["3RW4745-0LC00","Power semiconductor module 690 V, for 3RW4444/4445, 313 A two units for each device",895,"ST",1,"CP",1.3149999999999999,1,"3RW47450LC00"]
["3RW4936-8VX30","Fan for SIRIUS soft starter 3RW405.-.BB3 3RW442.-.BC3., 3RW443.-.BC3 115 V AC",144,"ST",1,"CP",0.42199999999999999,1,"3RW49368VX30"]
["3RW5215-3TC14","SIRIUS soft starter 200-480 V 25 A, 110-250 V AC spring-type terminals Thermistor input",1080,"ST",1,"CP",3.1,1,"3RW52153TC14"]
["3RW5217-3TC15","SIRIUS soft starter 200-600 V 38 A, 110-250 V AC spring-type terminals Thermistor input",1490,"ST",1,"CP",3.1,1,"3RW52173TC15"]
["3RW5236-6TC14","SIRIUS soft starter 200-480 V 171 A, 110-250 V AC Screw terminals Thermistor input",3208,"ST",1,"CP",8.1,1,"3RW52366TC14"]
["3RW5246-2TC05","SIRIUS soft starter 200-600 V 370 A, 24 V AC/DC spring-type terminals Thermistor input",6719,"ST",1,"CP",11.2,1,"3RW52462TC05"]
["3RW5525-1HA06","SIRIUS soft starter 200-690 V 63 A, 24 V AC/DC Screw terminals",2888,"ST",1,"CP",10,1,"3RW55251HA06"]
["3RW5546-2HA04","SIRIUS soft starter 200-480 V 370 A, 24 V AC/DC spring-type terminals",9303,"ST",1,"CP",10,1,"3RW55462HA04"]
["3RW5983-0TC20","Terminal cover for 3RW55/52 Size 2 and 3",22.8,"ST",1,"CP",9.1999999999999998E-2,1,"3RW59830TC20"]
["3RX9816-0AA00","AS-Interface heavy gauge feeder from ASI flat cable without individual slits Customer side heavy gauge 11 Continuation via pins","On request","ST",1,"CP",0.02,1,"3RX98160AA00"]
["3SB2455-0E","Contact block, 1 NO, 1 NO, soldering pin connection",13.299999999999999,"ST",1,"CP",9.9999999999999995E-7,1,"3SB24550E"]
["3SE5000-0AA02","twist lever for position switch 3SE51 Metal lever Form A 27 mm long, Step 9 mm with Stainless steel roller 19 mm",12.4,"ST",1,"CP",0.03,1,"3SE50000AA02"]
["3SE5000-0AE05-1AJ0","Actuator head for position switch 3SE5132 Roller lever metal lever, with plastic roller 22 mm functional at -40 Β°C",27.400000000000002,"ST",1,"CP",2.5999999999999999E-2,1,"3SE50000AE051AJ0"]
["3SE5000-0CA00","Contact block for position switch 3SE51/52 1 NO/1 NC quick action contact",14,"ST",1,"CP",2.1000000000000001E-2,1,"3SE50000CA00"]
["3SE5114-0LH01-1AE3","Position switch with lever Metal enclosure 40 mm according to EN 50041, 1 NO/2 NC quick action contacts, with M12 connector, 5-pole, fixed pin assignment Pin1=21, Pin4=22 Pin2=31, Pin5=32, Pin3=PE. Rotary actuator right and/or left adjustable, metal lever 27 mm long and plastic roller 19 mm. Suitable for connection to all SIMATIC ET200* compact block I/O modules.",72.3,"ST",1,"CP",0.34699999999999998,1,"3SE51140LH011AE3"]
["3SE5122-0CH60","Position switch Metal enclosure 56 mm wide Device connection 3x (M20x 1.5) 1 NO/1 NC quick action contacts Rotary actuator right/left adjustable, with adjustable-length metal lever 100 mm long and with positive fit (grid hole) and plastic roller 19 mm",53.1,"ST",1,"CP",0.45800000000000002,1,"3SE51220CH60"]
["3SE5132-0CD05","Position switch Plastic enclosure 40 mm according to EN 50041 Device connection 1 x (M20 x 1.5) 1 NO/1 NC quick action contacts 1 NO/1 NC quick action contacts Roller plunger, Form C with Plastic roller 13 mm",30.200000000000003,"ST",1,"CP",0.13,1,"3SE51320CD05"]
["3SE5212-0AC05-1CA0","Empty enclosure for position switch made of metal with increased corrosion protection according to EN 50047, 31 mm M20 x 1.5 with cover Color turquoise and plunger",14.299999999999999,"ST",1,"CP",0.16400000000000001,1,"3SE52120AC051CA0"]
["3SE5212-3RV40","Safety position switch with separate actuator Metal enclosure 31 mm, 1x (M20x 1.5) Slow-action contacts 1 NO+1 NC 2x LED yellow/green 230 V AC 5 directions of approaches The matching separate Actuator 3SE5000-0AV0./-0AW. must be ordered separately",63.7,"ST",1,"CP",0.23499999999999999,1,"3SE52123RV40"]
["3SE5234-0KC05-1AE0","Position switch Plastic enclosure according to EN 50047, 31 mm 1 NO/2 NC slow-action contacts with M12 connector, 4-pole 2 NC connected Pin assignment: Pin1=21, Pin2=22 Pin3=31, Pin4=32 for max. 250 V and 4 A with Teflon plunger",38.700000000000003,"ST",1,"CP",7.6999999999999999E-2,1,"3SE52340KC051AE0"]
["3SE5312-2SG12","Safety position switch with tumbler Locking force 2600 N 5 directions of approaches Spring-locked Escape release from the rear and auxiliary release on front Magnet voltage 115 V AC Monitoring actuator 2 NC/1 NO Monitoring magnet 2 NC/1 NO LED display yellow/green Supplied without actuator. Actuator 3SE5000-0AV0. please order separately",350,"ST",1,"CP",1.107,1,"3SE53122SG12"]
["3SE5324-0SB21-1AP0","Safety position switch with tumbler locking force 1300 N, 5 directions of approach, solenoid-locked, magnet voltage 24 V DC, monitoring actuator 2 NC/1 NO monitoring magnet 2 NC/1 NO  wired with M12 connector, 8-pole. The head is mounted by 90Β° (clockwise). The matching actuator 3SE5000-0AV0. /-0AW.. must be ordered separately.",282,"ST",1,"CP",0.505,1,"3SE53240SB211AP0"]
["3SE7310-1AE00","Conveyor belt unbalance tracker Metal enclosure, 2 x M25 x 1.5 2 NO+2 NC, with latching according to EN ISO 13850 Pushbutton release",592,"ST",1,"CP",1.859,1,"3SE73101AE00"]
["3SK1121-1CB42","SIRIUS safety relay Basic unit Advanced series with time delay 0.5-30 s Relay enabling circuits 2 NO instantaneous 2 NO delayed Us = 24 V DC screw terminal",302,"ST",1,"CP",0.29299999999999998,1,"3SK11211CB42"]
["3SK2122-2AA10","SIRIUS safety relay Basic unit 3SK2 series 20 F-DI, 4 F-DQ, 2 DQ, 24 V DC Can be parameterized via SIRIUS Safety ES 45 mm overall width Spring-type terminal (push-in) up to SILCL 3 (DIN EN 62061) Up to Performance Level E (ISO 13849-1) Output expansions 3SK1 and fail-safe motor starters 3RM1 via device connector connectable",547,"ST",1,"CP",0.37,1,"3SK21222AA10"]
["3SU1000-4BN01-0AA0","RONIS key-operated switch, 22 mm, round, plastic, lock number SB30, with 2 keys, 3 switch positions I-O<II, left latching, right momentary contact type, actuating angle 2x45Β°, 10:30h/12h/13:30h, key removal O, possible special locks: SB31, 421, 455",22.8,"ST",1,"CP",0.02,1,"3SU10004BN010AA0"]
["3SU1000-5HF01-0AA0","key-operated switch CES, 22 mm, round, plastic, Lock No. LSG1, with 2 keys, 2 switch positions O-I, latching, actuating angle 90Β°, 10:30h/13:30h, Key removal O",53.6,"ST",1,"CP",0.02,1,"3SU10005HF010AA0"]
["3SU1001-0BB50-0AA0","Illuminated pushbutton, 22 mm, round, plastic, blue, pushbutton, raised momentary contact type",6.5,"ST",1,"CP",1.7999999999999999E-2,1,"3SU10010BB500AA0"]
["3SU1030-0AB10-0AA0","Pushbutton, 22 mm, round, plastic with metal front ring, black, pushbutton, flat momentary contact type",5,"ST",1,"CP",2.5000000000000001E-2,1,"3SU10300AB100AA0"]
["3SU1030-5BM01-0AA0","key-operated switch CES, 22 mm, round, plastic with metal front ring, lock number SSG10, with 2 keys, 3 switch positions I>O<II, momentary contact type, actuating angle 2x45Β°, 10:30h/12h/13:30h, Key removal O",51.800000000000004,"ST",1,"CP",0.02,1,"3SU10305BM010AA0"]
["3SU1030-5TF11-0AA0","Key-operated switch BKS, 22 mm, round, plastic with metal front ring, Lock No. E9 (VW), without key, 2 switch positions O-I, latching, actuating angle 90Β°, 10:30h/13:30h, Key removal O+I",68.8,"ST",1,"CP",0.125,1,"3SU10305TF110AA0"]
["3SU1050-0AB60-0AA0","Pushbutton, 22 mm, round, metal, shiny, white, pushbutton, flat momentary contact type",5.6,"ST",1,"CP",4.1000000000000002E-2,1,"3SU10500AB600AA0"]
["3SU1050-1HU10-0AA0","Mushroom pushbutton, 22 mm, round, metal, shiny, black, 40 mm, with CES lock, lock no. VL5, positive latching, acc. to EN ISO 13850, key-operated release",125,"ST",1,"CP",0.16,1,"3SU10501HU100AA0"]
["3SU1050-5BP01-0AA0","key-operated switch CES, 22 mm, round, metal, shiny, lock number SSG10, with 2 keys, 3 switch positions I>O<II, momentary contact on the left, latching on the right, actuating angle 2x45Β°, 10:30h/12h/13:30h, Key removal O",57.6,"ST",1,"CP",0.02,1,"3SU10505BP010AA0"]
["3SU1051-0AA40-0AA0","Illuminated pushbutton, 22 mm, round, metal, shiny, green, pushbutton, flat, latching, Push-to-release mechanism",11.299999999999999,"ST",1,"CP",0.04,1,"3SU10510AA400AA0"]
["3SU1052-2BM60-0AA1","Selector switch, illuminable, 22 mm, round, metal, shiny, white, selector switch, short, 3 switch positions I>O<II, momentary contact type, actuating angle 2x45Β°, 10:30h/12h/13:30h, ATEX",32.800000000000004,"ST",1,"CP",4.4999999999999998E-2,1,"3SU10522BM600AA1"]
["3SU1060-4LM01-0AA0","RONIS key-operated switch, 30 mm, round, metal, matte, front ring for flush installation, lock number SB30, with 2 keys, 3 switch positions I>O<II, momentary contact type, actuating angle 2x45Β°, 10:30h/12h/13:30h, key removal O, possible special locks: SB31, 421, 455",30.6,"ST",1,"CP",0.02,1,"3SU10604LM010AA0"]
["3SU1062-2DL60-0AA0","Selector switch, illuminable, 30 mm, round, metal, matte, white, selector switch, short, front ring for flush installation, 3 switch positions I-O-II, latching, actuating angle 2x45Β°, 10:30h/12h/13:30h",16.700000000000003,"ST",1,"CP",0.02,1,"3SU10622DL600AA0"]
["3SU1100-7BE10-1QA0","Coordinate switch, 22 mm, round, plastic, black, 4 switch positions, latching, with mechanical interlocking, in O position, with holder, 1 NO, 1 NO, 1 NO, 1 NO, screw terminal,",79.199999999999989,"ST",1,"CP",0.11,1,"3SU11007BE101QA0"]
["3SU1103-0AB60-3BA0","Illuminated pushbutton, 22 mm, round, plastic, white, pushbutton, flat, momentary contact type, with holder, 1 NO, LED module with integrated LED 110 V AC, Spring-type terminal",25.8,"ST",1,"CP",6.2E-2,1,"3SU11030AB603BA0"]
["3SU1132-0AB20-1BA0","Illuminated pushbutton, 22 mm, round, plastic with metal front ring, red, pushbutton, flat, momentary contact type, with holder, 1 NO, LED module with integrated LED 24 V AC/DC, screw terminal",20.100000000000001,"ST",1,"CP",6.5000000000000002E-2,1,"3SU11320AB201BA0"]
["3SU1150-0AB10-1CA0","Pushbutton, 22 mm, round, metal, shiny, black, pushbutton, flat, momentary contact type, with holder, 1 NC, screw terminal",12.1,"ST",1,"CP",9.2999999999999999E-2,1,"3SU11500AB101CA0"]
["3SU1152-0AB70-1FA0","Illuminated pushbutton, 22 mm, round, metal, shiny, clear, pushbutton, flat, momentary contact type, with holder, 1 NO+1 NC, LED module with integrated LED 24 V AC/DC, screw terminal",22.900000000000002,"ST",1,"CP",0.105,1,"3SU11520AB701FA0"]
["3SU1156-0AB50-1FA0","Illuminated pushbutton, 22 mm, round, metal, shiny, blue, pushbutton, flat, momentary contact type, with holder, 1 NO+1 NC, LED module with integrated LED 230 V AC, screw terminal",27.700000000000003,"ST",1,"CP",0.11,1,"3SU11560AB501FA0"]
["3SU1251-6AB70-1AA0","Indicator lights, compact, 22 mm, round, metal, clear, lens, smooth, with holder, Operating voltage 24 V AC/DC, screw terminal",10.9,"ST",1,"CP",8.4000000000000005E-2,1,"3SU12516AB701AA0"]
["3SU1400-1AA10-3DA0","Contact module with 2 contact elements, 2 NO, spring-type terminal, for front plate mounting",9.5,"ST",1,"CP",1.7999999999999999E-2,1,"3SU14001AA103DA0"]
["3SU1401-1BG20-3AA0","LED module with integrated LED 6-24V AC/DC red, spring-type terminal, for front plate mounting",8.6,"ST",1,"CP",1.2E-2,1,"3SU14011BG203AA0"]
["3SU1401-2BC20-1AA0","LED module with integrated LED 110 V AC, red, screw terminal, for floor mounting",13.6,"ST",1,"CP",8.0000000000000002E-3,1,"3SU14012BC201AA0"]
["3SU1401-3BA50-5AA0","LED module with integrated LED, blue, soldered connection, for use on printed circuit boards",6.6,"ST",1,"CP",4.0000000000000001E-3,1,"3SU14013BA505AA0"]
["3SU1803-0NG10-4RB1","AS-Interface enclosure for command devices, 22 mm, round, Enclosure material plastic, enclosure top part gray, 3 control points plastic, Recess for labels, C=EMERGENCY STOP mushroom pushbutton red, rotate-to-unlatch mechanism, illuminable, 1 NC, 1 NC, spring-type terminal, AS-Interface module fail-safe label, backing plate, B=Illuminated pushbutton yellow, 1 NC, spring-type terminal, AS-Interface module fail-safe A=Illuminated pushbutton white, 1 NC, LED module, spring-type terminal, labels glued in, floor mounting, M12 connector 4-po(*)",476,"ST",1,"CP",0.79300000000000004,1,"3SU18030NG104RB1"]
["3SU1900-0AF16-0GH0","Labeling plate for gluing on enclosure, label size 22x22 mm, black label, white font, with inscription: Gauche",1.8,"ST",1,"CP",3.0000000000000001E-3,10,"3SU19000AF160GH0"]
["3SU1900-0AF81-0AJ0","Labeling plate for gluing on enclosure, label size 22x22mm, silver label, black font, with inscription: Left",2.1,"ST",1,"CP",1E-3,10,"3SU19000AF810AJ0"]
["3SU1900-0BS10-0AA0","Label holder, flat, black, for 4 labeling plates 17.5 mm x 27 mm, for gluing",5.6,"ST",1,"CP",6.0000000000000001E-3,10,"3SU19000BS100AA0"]
["3SU1950-0FD80-0AA0","Key for key-operated switch BKS, Lock No. S1",8.7999999999999989,"ST",1,"CP",8.0000000000000002E-3,1,"3SU19500FD800AA0"]
["3TC4417-0BK2","Contactor, Size 2, 2-pole, DC-3 and 5, 32 A Auxiliary contacts 22 (2 NO + 2 NC) 120 V AC 50/60 Hz AC operation",205,"ST",1,"CP",0.68200000000000005,1,"3TC44170BK2"]
["3TC4817-0BB0","Contactor, Size 4, 2-pole, DC-3 and 5, 75 A Auxiliary switch 22 (2 NO + 2 NC) 24 V AC 50 Hz/29 V AC 60 Hz AC operation",816,"ST",1,"CP",3.4380000000000002,1,"3TC48170BB0"]
["3TC5217-0AN4","Contactor, Size 8, 2-pole, DC-3 and 5, 220 A Auxiliary switch 22 (2 NO + 2 NC) 250 V DC DC operation",1675,"ST",1,"CP",9.82,1,"3TC52170AN4"]
["3TF2001-7BB4","Contactor, Size 00, 3-pole, AC-3 4 kW/400 V; Flat connector terminal Auxiliary switch 01E (1 NC) 24 V DC DC operation Screw mounting (diagonal) !!! Phased-out product !!! Successor is SIRIUS 3RT201 or 3TG10",47.6,"ST",1,"CP",0.187,1,"3TF20017BB4"]
["3TF2010-0AM0","Contactor size S00, 3-pole AC-3 4 kW/400 V Screw terminal Auxiliary switch 10 E (1 NO) Alternating current operation 220 V AC 50 Hz/264 V AC 60 Hz !!! Phased-out product !!! Successor is SIRIUS 3RT201 or 3TG10",49.9,"ST",1,"CP",0.193,1,"3TF20100AM0"]
["3TF6933-1DF4","Contactor, Size 14, 3-pole, AC-3, 450 kW, 400/380 V (690 V) Auxiliary switch 33 (3 NO+3 NC) with reversing contactor 3TC4417-4A and series resistor DC economy circuit 110 V DC",4628,"ST",1,"CP",22.6,1,"3TF69331DF4"]
["3TH2022-0AG2","Contactor relay, 22E, EN 50011, 2 NO + 2 NC, Screw terminal AC operation 110 V AC 50/60 Hz !!! Phased-out product !!! Successor is SIRIUS 3RH21",50,"ST",1,"CP",0.19600000000000001,1,"3TH20220AG2"]
["3TH2031-0FB4","Contactor relay, 31E, EN 50011, 3 NO + 1 NC, Screw terminal Diode or varistor attachable 24 V DC DC operation, 1.2 W No additional auxiliary contacts !!! Phased-out product !!! Successor is SIRIUS 3RH21",55.7,"ST",1,"CP",0.215,1,"3TH20310FB4"]
["3TH2040-0AM6","Contactor relay, 40E, EN 50011, 4 NO; Screw terminal AC operation 220 V AC 60 Hz 200 V AC 50 Hz !!! Phased-out product !!! Successor is SIRIUS 3RH21",52.1,"ST",1,"CP",0.19500000000000001,1,"3TH20400AM6"]
["3TH2280-0AP0","Contactor relay, 80E, EN 50011, 8 NO; Screw terminal Width 45 mm 230 V AC 50 Hz, 277 V 60 Hz AC operation !!! Phased-out product !!! Successor is SIRIUS 3RH21",70.399999999999991,"ST",1,"CP",0.23200000000000001,1,"3TH22800AP0"]
["3TH4244-0BE4","Contactor relay, 44E, DIN EN 50011, 4NO + 4NC, screw terminal DC operation 60 V DC",126,"ST",1,"CP",0.66600000000000004,1,"3TH42440BE4"]
["3TH4253-0AL2","Contactor relay, 53E, DIN EN 50011, 5NO + 3NC, screw terminal AC operation 230 V AC 50/60 Hz",69.599999999999994,"ST",1,"CP",0.41699999999999998,1,"3TH42530AL2"]
["3TH4280-0BE4","Contactor relay, 80E, DIN EN 50011, 8 NO, screw terminal DC operation 60 V DC",126,"ST",1,"CP",0.66600000000000004,1,"3TH42800BE4"]
["3TH4355-0LF4","For contactor relays 55E, EN 50011 5 NO + 5 NC, screw terminal DC operation DC operation 110 V DC Integr. varistor",209,"ST",1,"CP",0.7,1,"3TH43550LF4"]
["3TH4373-0LB4","Contactor relay 100 E EN 50011 7 NO + 3 NC,screw terminal Direct current operation DC solenoid system Integrated varistor",205,"ST",1,"CP",0.71099999999999997,1,"3TH43730LB4"]
["3TK1742-0AV0","Contactor, AC-1, 4-pole, 1000 A, main contacts 4 NO, Auxiliary contacts 2 NO + 2 NC, AC operation 400...415 V AC 50 Hz",4889,"ST",1,"CP",20.100000000000001,1,"3TK17420AV0"]
["3TK2022-0BB4","Miniature contactor, Screw terminal, 2 NO + 2 NC Snap-on mounting standard mounting rail 24 VDC DC operation !!! Phased-out product !!! Successor is SIRIUS 3RT23/25",54.1,"ST",1,"CP",0.21299999999999999,1,"3TK20220BB4"]
["3TK2031-6AB0","Miniature contactor, soldering pin connection, 3 NO + 1 NC Screw mounting (diagonal) 24 V AC 50 Hz/29 V AC 60 Hz AC operation !!! Phased-out product !!! Successor is SIRIUS 3RT23/25",39.4,"ST",1,"CP",0.14899999999999999,1,"3TK20316AB0"]
["3TK2827-2AJ21","SIRIUS safety relay with relay enabling circuits (EC) 115 V AC, 45 mm overall width Spring-type terminal EC instantaneous: 2 NO EC delayed: 2NO, 0.05...3 s SC: 1NC monitored start Basic device Maximum achieved SIL: 3/2, PL: e/d","On request","ST",1,"CP",0.58899999999999997,1,"3TK28272AJ21"]
["3TK2845-1FB42","!!! Phased-out product !!! The successor product series is 3SK2 (see FAQ xxxxxxxxx) SIRIUS safety relay with relay and electronic 24 V DC, 45 mm screw terminal EC instantaneous: 2 NO EC delayed: 1 SC: 1 Spring-locked tumbler Basic device Maximum achievable PL according to EN 13849-1: Maximum achievable SIL according to IEC 61508: 3","On request","ST",1,"CP",0.40899999999999997,1,"3TK28451FB42"]
["3TX4422-2B","Auxiliary switch block, with flat connector terminal for contactor relays and motor contactors EN 50005 Ident. no. 22, 2 NO + 2 NC",24.200000000000003,"ST",1,"CP",0.04,1,"3TX44222B"]
["3TX7004-1LB02","Output coupling link Phased-out product !!! For further information, please contact our sales department screw terminal 1 CO hard gold-plated 24 V AC/DC Enclosure width 6.2 mm","On request","ST",1,"CP",3.4000000000000002E-2,1,"3TX70041LB02"]
["3TX7680-1A","Set of cables for Main circuit for 3TD68 04",780,"ST",1,"CP",4.0449999999999999,1,"3TX76801A"]
["3TY1304-1F","Series resistor 4 kohm",32.5,"ST",1,"CP",3.6999999999999998E-2,1,"3TY13041F"]
["3TY6483-0BW4","Magnet coil for contactor 3TB47, 3TB48, 3TC48, 48 V DC",150,"ST",1,"CP",1.0649999999999999,1,"3TY64830BW4"]
["3TY7403-0AK2","Magnet coil for contactors 3TF30-33, 3TF40-43, 3TH3, 3TH4 3TB40...44, 3TC44, 3TH8 120 V AC 50/60 Hz Replacement for 3TY4803-0AK1",19.100000000000001,"ST",1,"CP",6.8000000000000005E-2,1,"3TY74030AK2"]
["3TY7483-0AP6","Magnet coil for contactors 3TF48/49 and 3TK48 240 V AC 60 Hz/220 V AC 50 Hz",154,"ST",1,"CP",0.2,1,"3TY74830AP6"]
["3TY7503-0DY80-0AF7","Magnet coil for contactors 3TF50/51 and 3TK50 DC economy circuit 74 V DC","On request","ST",1,"CP",0.32700000000000001,1,"3TY75030DY800AF7"]
["3TY7563-0AP0","Magnet coil for contactors 3TF56 and 3TK56 230 V AC 50 Hz/277 V AC 60 Hz",138,"ST",1,"CP",0.89500000000000002,1,"3TY75630AP0"]
["3TY7693-0CM7","Magnet coil for contactor 3TF6944-.C.., 200...240 V AC 50/60 Hz",841,"ST",1,"CP",1.7849999999999999,1,"3TY76930CM7"]
["3UF7020-1AU01-0","Basic unit SIMOCODE pro S, PROFIBUS DP interface 1.5 Mbit/s, 4I/2O freely parameterizable, Us: 110...240 V AC/DC, input for thermistor connection Monostable relay outputs, expandable by a multifunctional module",380,"ST",1,"CP",0.253,1,"3UF70201AU010"]
["3UG4617-1CR20","Digital monitoring relay 3-phase supply voltage Autom. phase sequence correction Phase failure 3 x 160 to 690 V 50 to 60 Hz AC Undervoltage and overvoltage 160-690 V Hysteresis 1-20 V OFF delay 0-20 s Asymmetry 0-20% 1 CO for phase correction 1 CO for line supply faults screw terminal",197,"ST",1,"CP",0.15,1,"3UG46171CR20"]
["3UX1220","Power strips can handle up to 200 A for 3TE48/3UA62 Consisting of 3 power strips",36.300000000000004,"ST",1,"CP",7.2999999999999995E-2,1,"3UX1220"]
["4AM2342-4TN00-0EB0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,025 /0; UPRI(V):230+/-5%; USEC(V):24; ISEC(A):1,04; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:MOUNTING RAILS; EN 61558-2-6 >UL/CSA-RECOGNIZED< >SAFETY ISOLATING TRANSFORMER<",97,"ST",1,"CP",1.5,1,"4AM23424TN000EB0"]
["4AM3242-5AT10-0FA2","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,063 /0,192; UPRI(V):400+/-5%; USEC(V):230; ISEC(A):0,274; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREWS/MOUNTING RAILS; EN 61558-2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",157,"ST",1,"CP",2.2999999999999998,1,"4AM32425AT100FA2"]
["4AM4342-4TJ10-0FA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,315 /1,12; UPRI(V):230+/-5%; USEC(V):110; ISEC(A):2,86; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",243,"ST",1,"CP",5.4,1,"4AM43424TJ100FA0"]
["4AM4842-5AT10-0FA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,5 /2; UPRI(V):400+/-5%; USEC(V):230; ISEC(A):2,17; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",313,"ST",1,"CP",7.36,1,"4AM48425AT100FA0"]
["4AM5542-5MT10-0FA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,8 /3,4; UPRI(V):690+/-5%; USEC(V):230; ISEC(A):3,478; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",443,"ST",1,"CP",12.15,1,"4AM55425MT100FA0"]
["4AM5742-5MT10-0FA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):1 /5; UPRI(V):690+/-5%; USEC(V):230; ISEC(A):4,348; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-2 >CONTROL CIRCUIT TRANSFORMER<",542,"ST",1,"CP",15.15,1,"4AM57425MT100FA0"]
["4AP3042-8BC40-0HC0","TRANSFORMER SITAS; PHASES:3; PN/PN(S6)(KVA):3,2 /20; UPRI(V):Y500-400/D289-230; USEC(V):Y 400 / D 230; ISEC(A):4,6-8,0; F(HZ):50...60; VECTOR GR./SHIELD WNG.:IIIIII0 /0; TA/ISOKL:40 /B; IP23; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",2947,"ST",1,"CP",66.2,1,"4AP30428BC400HC0"]
["4AT3912-8DD40-0FD0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):6,3 /31,1; UPRI(V):550-525-500-480-460- 440-415-400-380-230-208; USEC(V):2X115; ISEC(A):2X27,4; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:55 /H; IP54; TYPE OF TERMINALS:SCREW CONNECTION; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",3816,"ST",1,"CP",103,1,"4AT39128DD400FD0"]
["4AV4103-2EB00-0A","POWER SUPPLY; PHASES:1; PN(KW):0,072; UPRI(V):400-230+/-15; USEC(V DC):24; ISEC(A DC):3; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; PROTECTION CL.:I; TA/ISOKL:40 /B; W(%):5; IP00; TYPE OF TERMINALS:SCREW CONNECTION; INSTALLATION:SCREWS/MOUNTING RAILS; EN 61558, EN61131-2 >SAFETY ISOLATING TRANSFORMER<",288,"ST",1,"CP",2.66,1,"4AV41032EB000A"]
["4EU2452-4UA00-0AA0","MAINS CHOKE F.FU; PHASES:3; UN1(V):480; ITHMAX 1(A) / F1(HZ):80 /60; I LN (A):72; UK(%):4; LN(MH):0,352; TA/ISOKL:40 /H; IP00; TYPE OF TERMINALS:FLAT-TYPE TERMINAL; EN 61558-2-20 >UL/CSA-RECOGNIZED< >CHOKE<",2063,"ST",1,"CP",12.15,1,"4EU24524UA000AA0"]
["8WD4240-5AD","Continuous light element, with integrated LED, yellow, 115 V AC, Diameter 50 mm",89,"ST",1,"CP",5.5E-2,1,"8WD42405AD"]
["8WD4348-1XX","incandescent lamp, 115 V AC, 5 W, Base BA 15d, accessory for signaling columns, with diameters 50 mm + 70 mm, (Packing unit 10 units)",7.1999999999999993,"ST",1,"CP",8.0000000000000002E-3,10,"8WD43481XX"]
["8WD4440-5AB","Continuous light element, with integrated LED, red, 115 V AC, Diameter 70 mm",71.5,"ST",1,"CP",7.3999999999999996E-2,1,"8WD44405AB"]
["LZX:PT270615","Plug-in relay, 2 change-over contacts 115 V AC, also for LZS sockets",6.3999999999999995,"ST",1,"CP",3.1E-2,1,"LZX:PT270615"]
["3RK1901-1KA01","AS-Interface accessory Cover M12 for module IP67 tamper-proof design outer diameter 15 mm, with O-ring",154,"ST",100,"CP",8.0000000000000004E-4,10,"3RK19011KA01"]
["3RK1901-1MD00","AS-Interface accessory Profile seal for cable gland M20 x 1.5 for AS-i cable, shaped",220,"ST",100,"CP",2E-3,10,"3RK19011MD00"]
["3RK1901-1PN00","AS-Interface accessory Cover M8 for module IP67",159,"ST",100,"CP",5.2999999999999998E-4,10,"3RK19011PN00"]
["3RK1901-3QA00","AS-Interface accessory Cable clip for cable adapter EC",187,"ST",100,"CP",1E-3,10,"3RK19013QA00"]
["3RK1902-0AR00","AS-Interface accessory Sealing for mounting plate for sealing the enclosure for only single-sided entry of the shaped cables consists of 2 seals (1 straight + 1 shaped)",165,"ST",100,"CP",1E-3,5,"3RK19020AR00"]
["3RQ3902-0A","clip-on label 5 x 5 mm",9.6,"ST",100,"CP",8.9999999999999992E-5,2000,"3RQ39020A"]
["3RQ3902-0B","clip-on label 6 x 12 mm",21.6,"ST",100,"CP",1.7199999999999998E-4,1200,"3RQ39020B"]
["3RT1900-1SB10","Identification labels 10 x 7 mm RAL 6034 consists of 17 frames 48 labels per frame =816 labels ! Phased-out product! Successor is SIRIUS 3RT2","On request","ST",100,"CP",2.7E-4,816,"3RT19001SB10"]
["3RT1900-1SB20","Identification labels 20 x 7 mm pastel-turquoise consists of 340 labels on frame 20 labels per frame ! Phased-out product! Successor is SIRIUS 3RT2","On request","ST",100,"CP",6.2E-4,340,"3RT19001SB20"]
["3RT1900-1SB30","Identification labels 11 x 22 mm pastel-turquoise center latching (1 pack = 50 labels) ! Phased-out product! Successor is SIRIUS 3RT2","On request","ST",100,"CP",1E-3,50,"3RT19001SB30"]
["3RT1900-1SB50","Labeling plates for SIRIUS Net 20 x 9 pastel-turquoise (19 frames with 20 labels each) ! Phased-out product! Successor is SIRIUS 3RT2","On request","ST",100,"CP",8.1599999999999999E-4,380,"3RT19001SB50"]
["3RT1900-1SB60","Adhesive labels 19 x 6 mm, pastel-turquoise comprises 10 sheets A4 with 306 labels each ! Phased-out product! Successor is SIRIUS 3RT2","On request","ST",100,"CP",0.153,3060,"3RT19001SB60"]
["3RT1900-1SD60","Adhesive labels 19 x 6 mm, zinc-yellow comprises 10 sheets A4 with 306 labels each ! Phased-out product! Successor is SIRIUS 3RT2","On request","ST",100,"CP",5.1999999999999997E-5,3060,"3RT19001SD60"]
["3RT2900-1SB10","Labeling plates 10x7 mm Titanium gray Box contains 17 mats 48 labels per mat 816 labels",10.7,"ST",100,"CP",2.6400000000000002E-4,816,"3RT29001SB10"]
["3RT2900-1SB20","Labeling plates 20x7 mm Ti - gray Box contains 17 mats on mats 20 labels per mat",23.700000000000003,"ST",100,"CP",6.1799999999999995E-4,340,"3RT29001SB20"]
["3RT2900-1SB60","Adhesive labels 19x6 mm Titanium gray comprises 10 sheets DIN A4 306 labels each = 3060 units",2.2000000000000002,"ST",100,"CP",5.1E-5,3060,"3RT29001SB60"]
["3RT2916-4PA00","Combination bolt set 100 units for contactors size S00",82.1,"ST",100,"CP",0.123,100,"3RT29164PA00"]
["3RT2926-4PA00","Combination bolt set = 100 units for motor contactor ring cable lug Size S0, M3 for auxiliary current path",86.399999999999991,"ST",100,"CP",8.5999999999999998E-4,100,"3RT29264PA00"]
["3RT2926-4PA01","Combination bolt set = 100 units for motor contactor ring cable lug Size S0, M4 main circuit",86.399999999999991,"ST",100,"CP",2E-3,100,"3RT29264PA01"]
["3RV1908-0P","Scale cover, sealable for circuit breaker Size S00...S3",85.899999999999991,"ST",100,"CP",6.6E-4,10,"3RV19080P"]
["3RV1908-0PA00-0FB0","Scale cover, sealable for circuit breaker Size S0...S3 ABB",85.899999999999991,"ST",100,"CP",7.0000000000000001E-3,10,"3RV19080PA000FB0"]
["3RV2908-0P","scale cover, sealable for circuit breaker 3RV2 Size S00...S3",80.899999999999991,"ST",100,"CP",5.1000000000000004E-4,10,"3RV29080P"]
["3RV2917-6A","End cover for 3-phase busbar 3RV2917 Multi-unit packaging 10 units",59.4,"ST",100,"CP",6.0000000000000001E-3,10,"3RV29176A"]
["3RV2928-0B","Push-in lug size S00/S0",28.5,"ST",100,"CP",2E-3,10,"3RV29280B"]
["3RX9802-0AA00","AS-Interface accessory Cover M12 for module IP67 outer diameter 12 mm, without O-ring",152,"ST",100,"CP",7.1999999999999994E-4,10,"3RX98020AA00"]
["3RX9805-0AA00","AS-Interface accessory Seal PG11 for AS-i cable, shaped",243,"ST",100,"CP",2E-3,10,"3RX98050AA00"]
["3SB2901-2AA","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, without inscription for self-labeling",57,"ST",100,"CP",4.7999999999999996E-4,10,"3SB29012AA"]
["3SB2901-2AB","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, with inscription: In",80.5,"ST",100,"CP",0.48,10,"3SB29012AB"]
["3SB2901-2AC","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, with inscription: Off",80.5,"ST",100,"CP",4.7999999999999996E-4,10,"3SB29012AC"]
["3SB2901-2AD","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, with inscription: Up",80.5,"ST",100,"CP",4.7999999999999996E-4,10,"3SB29012AD"]
["3SB2901-2AF","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, with inscription: Forward",80.5,"ST",100,"CP",4.7999999999999996E-4,10,"3SB29012AF"]
["3SB2901-2AG","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, with inscription: Back",80.5,"ST",100,"CP",4.7999999999999996E-4,10,"3SB29012AG"]
["3SB2901-2AL","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, with inscription: Close",80.5,"ST",100,"CP",4.7999999999999996E-4,10,"3SB29012AL"]
["3SB2901-2AM","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, with inscription: fast",80.5,"ST",100,"CP",4.7999999999999996E-4,10,"3SB29012AM"]
["3SB2901-2AN","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, with inscription: Left",80.5,"ST",100,"CP",4.7999999999999996E-4,10,"3SB29012AN"]
["3SB2901-2AP","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, with inscription: operation",80.5,"ST",100,"CP",4.7999999999999996E-4,10,"3SB29012AP"]
["3SB2901-2AQ","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, with inscription: Fault",80.5,"ST",100,"CP",4.7999999999999996E-4,10,"3SB29012AQ"]
["3SB2901-2AR","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, with inscription: set-up",80.5,"ST",100,"CP",4.7999999999999996E-4,10,"3SB29012AR"]
["3SB2901-2BA","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, with inscription: Manual Auto",80.5,"ST",100,"CP",4.7999999999999996E-4,10,"3SB29012BA"]
["3SB2901-2BE","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, with inscription: Manual O Auto",80.5,"ST",100,"CP",4.7999999999999996E-4,10,"3SB29012BE"]
["3SB2901-2EB","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, with inscription: Right",80.5,"ST",100,"CP",4.7999999999999996E-4,10,"3SB29012EB"]
["3SB2901-2EC","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, with inscription: Off",80.5,"ST",100,"CP",4.7999999999999996E-4,10,"3SB29012EC"]
["3SB2901-2EL","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, with inscription: start",80.5,"ST",100,"CP",4.7999999999999996E-4,10,"3SB29012EL"]
["3SB2901-2EM","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, with inscription: Reset",80.5,"ST",100,"CP",4.7999999999999996E-4,10,"3SB29012EM"]
["3SB2901-2ET","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, with inscription: Manual O Auto",80.5,"ST",100,"CP",4.7999999999999996E-4,10,"3SB29012ET"]
["3SB2901-2EW","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, with inscription: Fault",80.5,"ST",100,"CP",4.7999999999999996E-4,10,"3SB29012EW"]
["3SB2901-2MB","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, with graphic symbol: O",80.5,"ST",100,"CP",4.7999999999999996E-4,10,"3SB29012MB"]
["3SB2901-2MC","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, with graphic symbol: I",80.5,"ST",100,"CP",4.7999999999999996E-4,10,"3SB29012MC"]
["3SB2901-2MF","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, with graphic symbol: O I",80.5,"ST",100,"CP",4.7999999999999996E-4,10,"3SB29012MF"]
["3SB2901-2NA","Adhesive labeling plate, on label holder, Label size 9.5 x 18.5 mm, silver-colored, black font, with graphic symbol: In",80.5,"ST",100,"CP",4.7999999999999996E-4,10,"3SB29012NA"]
["3SB2901-4AA","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, without inscription, for self-labeling",57,"ST",100,"CP",1E-4,10,"3SB29014AA"]
["3SB2901-4AB","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with inscription: In",80.5,"ST",100,"CP",2E-3,10,"3SB29014AB"]
["3SB2901-4AC","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with inscription: Off",80.5,"ST",100,"CP",2E-3,10,"3SB29014AC"]
["3SB2901-4AD","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with inscription: Up",80.5,"ST",100,"CP",2E-3,10,"3SB29014AD"]
["3SB2901-4AE","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with inscription: Down",80.5,"ST",100,"CP",2E-3,10,"3SB29014AE"]
["3SB2901-4AF","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with inscription: Forward",80.5,"ST",100,"CP",2E-3,10,"3SB29014AF"]
["3SB2901-4AG","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with inscription: Back",80.5,"ST",100,"CP",2E-3,10,"3SB29014AG"]
["3SB2901-4AH","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with inscription: Right",80.5,"ST",100,"CP",2E-3,10,"3SB29014AH"]
["3SB2901-4AJ","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with inscription: Left",80.5,"ST",100,"CP",2E-3,10,"3SB29014AJ"]
["3SB2901-4AK","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with inscription: Stop",80.5,"ST",100,"CP",2E-3,10,"3SB29014AK"]
["3SB2901-4AL","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with inscription: Close",80.5,"ST",100,"CP",2E-3,10,"3SB29014AL"]
["3SB2901-4AN","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with inscription: slow",80.5,"ST",100,"CP",2E-3,10,"3SB29014AN"]
["3SB2901-4AQ","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with inscription: Fault",80.5,"ST",100,"CP",2E-3,10,"3SB29014AQ"]
["3SB2901-4EB","Inscription plate for pushbutton and illuminated pushbutton, flat, milky with black font, with inscription: ON",80.5,"ST",100,"CP",2E-3,10,"3SB29014EB"]
["3SB2901-4EK","Inscription plate for pushbutton and illuminated pushbutton, flat, milky with black font, with inscription: START",80.5,"ST",100,"CP",2E-3,10,"3SB29014EK"]
["3SB2901-4EL","Inscription plate for pushbutton and illuminated pushbutton, flat, milky with black font, with inscription: STOP",80.5,"ST",100,"CP",2E-3,10,"3SB29014EL"]
["3SB2901-4EM","Inscription plate for pushbutton and illuminated pushbutton, flat, milky with black font, with inscription: RESET",80.5,"ST",100,"CP",2E-3,10,"3SB29014EM"]
["3SB2901-4EN","Inscription plate for pushbutton and illuminated pushbutton, flat, milky with black font, with inscription: TEST",80.5,"ST",100,"CP",2E-3,10,"3SB29014EN"]
["3SB2901-4MB","Inscription plate for pushbutton and illuminated pushbutton, flat, milky with black font, with graphic symbol: O",80.5,"ST",100,"CP",2E-3,10,"3SB29014MB"]
["3SB2901-4MC","Inscription plate for pushbutton and illuminated pushbutton, flat, milky with black font, with graphic symbol: I",80.5,"ST",100,"CP",2E-3,10,"3SB29014MC"]
["3SB2901-4MD","Inscription plate for pushbutton and illuminated pushbutton, flat, milky with black font, with graphic symbol: II",80.5,"ST",100,"CP",2E-3,10,"3SB29014MD"]
["3SB2901-4NA","Inscription plate for pushbutton and illuminated pushbutton, flat, milky with black font, with graphic symbol: MOTION DIRECTION OF ARROW",80.5,"ST",100,"CP",2E-3,10,"3SB29014NA"]
["3SB2901-4NB","Inscription plate for pushbutton and illuminated pushbutton, flat, milky with black font, with graphic symbol: MOTION DIRECTION OF ARROW",80.5,"ST",100,"CP",2E-3,10,"3SB29014NB"]
["3SB2901-4NC","Inscription plate for pushbutton and illuminated pushbutton, flat, milky with black font, with graphic symbol: ROTATION TO THE RIGHT",80.5,"ST",100,"CP",2E-3,10,"3SB29014NC"]
["3SB2901-4ND","Inscription plate for pushbutton and illuminated pushbutton, flat, milky with black font, with graphic symbol: ROTATION TO THE LEFT",80.5,"ST",100,"CP",2E-3,10,"3SB29014ND"]
["3SB2901-4NE","Inscription plate for pushbutton and illuminated pushbutton, flat, milky with black font, with graphic symbol: RAPID TRAVERSE",80.5,"ST",100,"CP",2E-3,10,"3SB29014NE"]
["3SB2901-4NG","Inscription plate for pushbutton and illuminated pushbutton, flat, milky with black font, with graphic symbol: INCREASE, PLUS",80.5,"ST",100,"CP",2E-3,10,"3SB29014NG"]
["3SB2901-4PA","Inscription plate for pushbutton and illuminated pushbutton, flat, milky with black font, with graphic symbol: ELECTRIC MOTOR",80.5,"ST",100,"CP",2E-3,10,"3SB29014PA"]
["3SB2901-4PB","Inscription plate for pushbutton and illuminated pushbutton, flat, milky with black font, with graphic symbol: HORN",80.5,"ST",100,"CP",2E-3,10,"3SB29014PB"]
["3SB2901-4PD","Inscription plate for pushbutton and illuminated pushbutton, flat, milky with black font, with graphic symbol: PUMP",80.5,"ST",100,"CP",2E-3,10,"3SB29014PD"]
["3SB2901-4PE","Inscription plate for pushbutton and illuminated pushbutton, flat, milky with black font, with graphic symbol: COOLANT PUMP",80.5,"ST",100,"CP",2E-3,10,"3SB29014PE"]
["3SB2901-4QB","Inscription plate for pushbutton and illuminated pushbutton, flat, milky with black font, with graphic symbol: CLAMP",80.5,"ST",100,"CP",2E-3,10,"3SB29014QB"]
["3SB2901-4QC","Inscription plate for pushbutton and illuminated pushbutton, flat, milky with black font, with graphic symbol: RELEASE",80.5,"ST",100,"CP",2E-3,10,"3SB29014QC"]
["3SB2901-4QE","Inscription plate for pushbutton and illuminated pushbutton, flat, milky with black font, with graphic symbol: RELEASE BRAKE",80.5,"ST",100,"CP",2E-3,10,"3SB29014QE"]
["3SB2901-4QF","Inscription plate for pushbutton and illuminated pushbutton, flat, milky with black font, with graphic symbol: LOCK",80.5,"ST",100,"CP",2E-3,10,"3SB29014QF"]
["3SB2901-4QG","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with graphic symbol: unlock",80.5,"ST",100,"CP",2E-3,10,"3SB29014QG"]
["3SB2901-4QJ","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with graphic symbol: on/off momentary contact",80.5,"ST",100,"CP",2E-3,10,"3SB29014QJ"]
["3SB2901-4QK","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with graphic symbol: manual operation",80.5,"ST",100,"CP",2E-3,10,"3SB29014QK"]
["3SB2901-4QL","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with graphic symbol: automatic sequence",80.5,"ST",100,"CP",2E-3,10,"3SB29014QL"]
["3SB2901-4RA","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with graphic symbol: 0",80.5,"ST",100,"CP",2E-3,10,"3SB29014RA"]
["3SB2901-4RB","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with graphic symbol: 1",80.5,"ST",100,"CP",2E-3,10,"3SB29014RB"]
["3SB2901-4RC","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with graphic symbol: 2",80.5,"ST",100,"CP",2E-3,10,"3SB29014RC"]
["3SB2901-4RD","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with graphic symbol: 3",80.5,"ST",100,"CP",2E-3,10,"3SB29014RD"]
["3SB2901-4RE","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with graphic symbol: 4",80.5,"ST",100,"CP",2E-3,10,"3SB29014RE"]
["3SB2901-4RF","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with graphic symbol: 5",80.5,"ST",100,"CP",2E-3,10,"3SB29014RF"]
["3SB2901-4RG","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with graphic symbol: 6",80.5,"ST",100,"CP",2E-3,10,"3SB29014RG"]
["3SB2901-4RH","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with graphic symbol: 7",80.5,"ST",100,"CP",2E-3,10,"3SB29014RH"]
["3SB2901-4RJ","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with graphic symbol: 8",80.5,"ST",100,"CP",2E-3,10,"3SB29014RJ"]
["3SB2901-4RK","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with graphic symbol: 9",80.5,"ST",100,"CP",2E-3,10,"3SB29014RK"]
["3SB2901-5AA","Insert cap for pushbutton and illuminated pushbutton raised, clear, without inscription, for self-labeling",80.5,"ST",100,"CP",4.3399999999999998E-4,10,"3SB29015AA"]
["3SB2901-5AB","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with inscription: In",102,"ST",100,"CP",2E-3,10,"3SB29015AB"]
["3SB2901-5AC","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with inscription: Off",102,"ST",100,"CP",2E-3,10,"3SB29015AC"]
["3SB2901-5AD","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with inscription: Up",102,"ST",100,"CP",2E-3,10,"3SB29015AD"]
["3SB2901-5AF","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with inscription: Forward",102,"ST",100,"CP",2E-3,10,"3SB29015AF"]
["3SB2901-5AG","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with inscription: Back",102,"ST",100,"CP",2E-3,10,"3SB29015AG"]
["3SB2901-5AL","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with inscription: Close",102,"ST",100,"CP",2E-3,10,"3SB29015AL"]
["3SB2901-5EB","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with inscription: On",102,"ST",100,"CP",1E-3,10,"3SB29015EB"]
["3SB2901-5MB","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with graphic symbol: O",102,"ST",100,"CP",2E-3,10,"3SB29015MB"]
["3SB2901-5MC","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with graphic symbol: I",102,"ST",100,"CP",2E-3,10,"3SB29015MC"]
["3SB2901-5MD","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with graphic symbol: II",102,"ST",100,"CP",1E-3,10,"3SB29015MD"]
["3SB2901-5NA","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with graphic symbol: Motion direction of arrow",102,"ST",100,"CP",2E-3,10,"3SB29015NA"]
["3SB2901-5NB","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with graphic symbol: Motion direction of arrow",102,"ST",100,"CP",2E-3,10,"3SB29015NB"]
["3SB2901-5NG","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with graphic symbol: Increase, Plus",102,"ST",100,"CP",2E-3,10,"3SB29015NG"]
["3SB2901-5QB","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with graphic symbol: clamp",102,"ST",100,"CP",2E-3,10,"3SB29015QB"]
["3SB2901-5QC","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with graphic symbol: release",102,"ST",100,"CP",2E-3,10,"3SB29015QC"]
["3SB2901-5QG","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with graphic symbol: unlock",102,"ST",100,"CP",2E-3,10,"3SB29015QG"]
["3SB2901-5QL","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with graphic symbol: automatic sequence",102,"ST",100,"CP",2E-3,10,"3SB29015QL"]
["3SB2901-5RA","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with graphic symbol: 0",102,"ST",100,"CP",2E-3,10,"3SB29015RA"]
["3SB2901-5RB","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with graphic symbol: 1",102,"ST",100,"CP",2E-3,10,"3SB29015RB"]
["3SB2901-5RC","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with graphic symbol: 2",102,"ST",100,"CP",2E-3,10,"3SB29015RC"]
["3SB2901-5RD","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with graphic symbol: 3",102,"ST",100,"CP",2E-3,10,"3SB29015RD"]
["3SB2901-5RE","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with graphic symbol: 4",102,"ST",100,"CP",2E-3,10,"3SB29015RE"]
["3SB2901-5RF","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with graphic symbol: 5",102,"ST",100,"CP",2E-3,10,"3SB29015RF"]
["3SB2901-5RG","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with graphic symbol: 6",102,"ST",100,"CP",2E-3,10,"3SB29015RG"]
["3SB2901-5RH","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with graphic symbol: 7",102,"ST",100,"CP",2E-3,10,"3SB29015RH"]
["3SB2901-5RJ","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with graphic symbol: 8",102,"ST",100,"CP",2E-3,10,"3SB29015RJ"]
["3SB2901-5RK","Insert cap for pushbutton and illuminated pushbutton raised, clear with black font, with graphic symbol: 9",102,"ST",100,"CP",2E-3,10,"3SB29015RK"]
["3SB2901-7AA","Insert cap for indicator light, clear with black font, without inscription, for self-labeling",80.5,"ST",100,"CP",3.2000000000000003E-4,10,"3SB29017AA"]
["3SB2901-7AP","Insert cap for indicator light, clear with black font, with inscription: operation",102,"ST",100,"CP",2E-3,1,"3SB29017AP"]
["3SB2901-7AQ","Insert cap for indicator light, clear with black font, with inscription: Fault",102,"ST",100,"CP",2E-3,10,"3SB29017AQ"]
["3SB2901-7PD","Insert cap for indicator light, clear with black font, with graphic symbol: Pump",102,"ST",100,"CP",2E-3,10,"3SB29017PD"]
["3SB2901-7QK","Insert cap for indicator light, clear with black font, with graphic symbol: manual operation",102,"ST",100,"CP",2E-3,10,"3SB29017QK"]
["3SB2902-0AA","Single frame of square design",33.200000000000003,"ST",100,"CP",9.59E-4,10,"3SB29020AA"]
["3SB2902-0AB","Label holder for labeling plate, Label size 9.5 x 18.5 mm,",58,"ST",100,"CP",9.9999999999999995E-7,10,"3SB29020AB"]
["3SB2908-1AA","incandescent lamp, clear, rated voltage 6 V AC/DC, 1.0 W, Wedge base W2 x 4.6 d,",102,"ST",100,"CP",1E-3,10,"3SB29081AA"]
["3SB2908-1AB","incandescent lamp, clear, rated voltage 12 V AC/DC, 1.0 W, Wedge base W2 x 4.6 d,",102,"ST",100,"CP",6.0999999999999997E-4,10,"3SB29081AB"]
["3SB2908-1AC","incandescent lamp, clear, rated voltage 24 V AC/DC, 1.0 W Wedge base W2 x 4.6 d,",102,"ST",100,"CP",5.5000000000000003E-4,10,"3SB29081AC"]
["3SB2908-1AD","incandescent lamp, clear, rated voltage 30 V AC/DC, 1.0 W, Wedge base W2 x 4.6 d,",102,"ST",100,"CP",6.1299999999999994E-4,10,"3SB29081AD"]
["3SB2908-8AA","Push-on contact for flat connector, 2.8 x 0.8 mm, Cross-section 0.5...1.5 mm2",18.5,"ST",100,"CP",2.3499999999999999E-4,250,"3SB29088AA"]
["3SB2908-8AB","Insulating sleeve for flat connector, 2.8 x 0.8 mm, can be plugged on from the front",18.5,"ST",100,"CP",2.0799999999999999E-4,250,"3SB29088AB"]
["3SB2908-8AE","Push-on contact for flat connector, 2.8 x 0.8 mm, with latch spring for latching into complete connector",23.900000000000002,"ST",100,"CP",3.1199999999999999E-4,10,"3SB29088AE"]
["3SB2910-0AB","pushbutton, white flat, for pushbutton",42.300000000000004,"ST",100,"CP",0.59,10,"3SB29100AB"]
["3SB2910-0AC","pushbutton, red, flat, for pushbutton",42.300000000000004,"ST",100,"CP",3.6999999999999999E-4,10,"3SB29100AC"]
["3SB2910-0AD","pushbutton, yellow, flat, for pushbutton",42.300000000000004,"ST",100,"CP",9.9999999999999995E-7,10,"3SB29100AD"]
["3SB2910-0AE","pushbutton, green, flat, for pushbutton",42.300000000000004,"ST",100,"CP",4.0000000000000002E-4,10,"3SB29100AE"]
["3SB2910-0AF","pushbutton, blue, flat, for pushbutton",42.300000000000004,"ST",100,"CP",9.9999999999999995E-7,10,"3SB29100AF"]
["3SB2910-0AG","pushbutton, white, flat, for pushbutton and illuminated pushbutton",42.300000000000004,"ST",100,"CP",9.3000000000000005E-4,10,"3SB29100AG"]
["3SB2910-0AH","pushbutton, clear, flat, for pushbutton and illuminated pushbutton",42.300000000000004,"ST",100,"CP",2.9999999999999997E-4,10,"3SB29100AH"]
["3SB2910-0CC","pushbutton, red, flat, for illuminated pushbutton",42.300000000000004,"ST",100,"CP",9.9999999999999995E-7,10,"3SB29100CC"]
["3SB2910-0CD","pushbutton, yellow, flat, for illuminated pushbutton",42.300000000000004,"ST",100,"CP",2.9999999999999997E-4,10,"3SB29100CD"]
["3SB2910-0CE","pushbutton, green, flat, for illuminated pushbutton",42.300000000000004,"ST",100,"CP",9.9999999999999995E-7,10,"3SB29100CE"]
["3SB2910-0CF","pushbutton, blue, flat, for illuminated pushbutton",42.300000000000004,"ST",100,"CP",4.0000000000000002E-4,10,"3SB29100CF"]
["3SB2910-1AC","lens, red, with concentric rings",42.300000000000004,"ST",100,"CP",6.4999999999999997E-4,10,"3SB29101AC"]
["3SB2910-1AD","lens, yellow, with concentric rings",42.300000000000004,"ST",100,"CP",5.9999999999999995E-4,10,"3SB29101AD"]
["3SB2910-1AE","lens, green, with concentric rings",42.300000000000004,"ST",100,"CP",2E-3,10,"3SB29101AE"]
["3SB2910-1AF","lens, blue, with concentric rings",42.300000000000004,"ST",100,"CP",8.0000000000000004E-4,10,"3SB29101AF"]
["3SB2910-1AG","lens, white, with concentric rings",42.300000000000004,"ST",100,"CP",7.6000000000000004E-4,10,"3SB29101AG"]
["3SB2910-1AH","lens, clear, with concentric rings",42.300000000000004,"ST",100,"CP",9.9999999999999995E-7,10,"3SB29101AH"]
["3SB2910-1BC","lens, red, smooth, for inscription with insert caps",42.300000000000004,"ST",100,"CP",9.9999999999999995E-7,10,"3SB29101BC"]
["3SB2910-1BD","lens, yellow, smooth, for inscription with insert caps",42.300000000000004,"ST",100,"CP",8.0000000000000004E-4,10,"3SB29101BD"]
["3SB2910-1BE","lens, green, smooth, for inscription with insert caps",42.300000000000004,"ST",100,"CP",9.9999999999999995E-7,10,"3SB29101BE"]
["3SB2910-1BF","lens, blue, smooth, for inscription with insert caps",42.300000000000004,"ST",100,"CP",9.9999999999999995E-7,10,"3SB29101BF"]
["3SB2910-1BH","lens, clear, smooth, for inscription with insert caps",42.300000000000004,"ST",100,"CP",9.9999999999999995E-7,10,"3SB29101BH"]
["3SU1900-0AB71-0AA0","Inscription plate for illuminated pushbutton, round, milky, without inscription, for self-labeling",74.5,"ST",100,"CP",4.1999999999999996E-4,10,"3SU19000AB710AA0"]
["3SU1900-0AB71-0AB0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: In",87.5,"ST",100,"CP",4.0000000000000002E-4,10,"3SU19000AB710AB0"]
["3SU1900-0AB71-0AC0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: Off",87.5,"ST",100,"CP",4.0000000000000001E-3,10,"3SU19000AB710AC0"]
["3SU1900-0AB71-0AD0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: Up",87.5,"ST",100,"CP",1E-3,10,"3SU19000AB710AD0"]
["3SU1900-0AB71-0AE0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: Down",87.5,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AB710AE0"]
["3SU1900-0AB71-0AF0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: Forward",87.5,"ST",100,"CP",1E-3,10,"3SU19000AB710AF0"]
["3SU1900-0AB71-0AG0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: Back",87.5,"ST",100,"CP",1E-3,10,"3SU19000AB710AG0"]
["3SU1900-0AB71-0AH0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: Right",87.5,"ST",100,"CP",4.0000000000000001E-3,10,"3SU19000AB710AH0"]
["3SU1900-0AB71-0AJ0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: Left",87.5,"ST",100,"CP",1E-3,10,"3SU19000AB710AJ0"]
["3SU1900-0AB71-0AK0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: Stop",87.5,"ST",100,"CP",1E-3,10,"3SU19000AB710AK0"]
["3SU1900-0AB71-0AL0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: Close",87.5,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AB710AL0"]
["3SU1900-0AB71-0AM0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: fast",87.5,"ST",100,"CP",1E-3,10,"3SU19000AB710AM0"]
["3SU1900-0AB71-0AN0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: slow",87.5,"ST",100,"CP",1E-3,10,"3SU19000AB710AN0"]
["3SU1900-0AB71-0AP0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: operation",87.5,"ST",100,"CP",1E-3,10,"3SU19000AB710AP0"]
["3SU1900-0AB71-0AQ0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: Fault",87.5,"ST",100,"CP",1E-3,10,"3SU19000AB710AQ0"]
["3SU1900-0AB71-0AR0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: set up",87.5,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AB710AR0"]
["3SU1900-0AB71-0DJ0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: On",74.5,"ST",100,"CP",8.0000000000000004E-4,10,"3SU19000AB710DJ0"]
["3SU1900-0AB71-0DK0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: Off",74.5,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AB710DK0"]
["3SU1900-0AB71-0DL0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: Up",74.5,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AB710DL0"]
["3SU1900-0AB71-0DM0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: Down",74.5,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AB710DM0"]
["3SU1900-0AB71-0DN0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: Forward",87.5,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AB710DN0"]
["3SU1900-0AB71-0DQ0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: Right",74.5,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AB710DQ0"]
["3SU1900-0AB71-0DR0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: Left",74.5,"ST",100,"CP",1E-3,10,"3SU19000AB710DR0"]
["3SU1900-0AB71-0DS0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: Stop",74.5,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AB710DS0"]
["3SU1900-0AB71-0DT0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: start",74.5,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AB710DT0"]
["3SU1900-0AB71-0DU0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: Reset",74.5,"ST",100,"CP",4.0000000000000002E-4,10,"3SU19000AB710DU0"]
["3SU1900-0AB71-0DV0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: test",87.5,"ST",100,"CP",1E-3,10,"3SU19000AB710DV0"]
["3SU1900-0AB71-0DW0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: Open",87.5,"ST",100,"CP",4.0000000000000002E-4,10,"3SU19000AB710DW0"]
["3SU1900-0AB71-0DX0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: Close",87.5,"ST",100,"CP",1.0000000000000001E-5,10,"3SU19000AB710DX0"]
["3SU1900-0AB71-0EB0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: Running",87.5,"ST",100,"CP",2E-3,10,"3SU19000AB710EB0"]
["3SU1900-0AB71-0EE0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: Fast",87.5,"ST",100,"CP",2E-3,10,"3SU19000AB710EE0"]
["3SU1900-0AB71-0EF0","Inscription plate for illuminated pushbutton, round, milky with black font, with inscription: Slow",87.5,"ST",100,"CP",1E-3,10,"3SU19000AB710EF0"]
["3SU1900-0AB71-0QA0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: O",74.5,"ST",100,"CP",4.6000000000000001E-4,10,"3SU19000AB710QA0"]
["3SU1900-0AB71-0QB0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: I",74.5,"ST",100,"CP",4.44E-4,10,"3SU19000AB710QB0"]
["3SU1900-0AB71-0QC0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: II",74.5,"ST",100,"CP",1E-3,10,"3SU19000AB710QC0"]
["3SU1900-0AB71-0QD0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: III",74.5,"ST",100,"CP",1E-3,10,"3SU19000AB710QD0"]
["3SU1900-0AB71-0QR0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: arrow pointing to the right",74.5,"ST",100,"CP",4.44E-4,10,"3SU19000AB710QR0"]
["3SU1900-0AB71-0QS0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: arrow pointing to the top left",74.5,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AB710QS0"]
["3SU1900-0AB71-0QT0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: rotation to the right",74.5,"ST",100,"CP",5.9899999999999992E-4,10,"3SU19000AB710QT0"]
["3SU1900-0AB71-0QU0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: rotation to the left",74.5,"ST",100,"CP",2.9999999999999997E-4,10,"3SU19000AB710QU0"]
["3SU1900-0AB71-0QV0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: Rapid traverse",87.5,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AB710QV0"]
["3SU1900-0AB71-0QW0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: feed",87.5,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AB710QW0"]
["3SU1900-0AB71-0QX0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: Increase, Plus",87.5,"ST",100,"CP",4.0000000000000001E-3,10,"3SU19000AB710QX0"]
["3SU1900-0AB71-0QY0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: decrease, minus",87.5,"ST",100,"CP",4.0000000000000002E-4,10,"3SU19000AB710QY0"]
["3SU1900-0AB71-0RA0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: electric motor",87.5,"ST",100,"CP",2E-3,10,"3SU19000AB710RA0"]
["3SU1900-0AB71-0RB0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: horn",87.5,"ST",100,"CP",2E-3,10,"3SU19000AB710RB0"]
["3SU1900-0AB71-0RC0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: water tap",87.5,"ST",100,"CP",1E-3,10,"3SU19000AB710RC0"]
["3SU1900-0AB71-0RD0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: pump",87.5,"ST",100,"CP",2E-3,10,"3SU19000AB710RD0"]
["3SU1900-0AB71-0RE0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: coolant pump",87.5,"ST",100,"CP",1E-3,10,"3SU19000AB710RE0"]
["3SU1900-0AB71-0RF0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: clamp",87.5,"ST",100,"CP",6.6700000000000006E-4,10,"3SU19000AB710RF0"]
["3SU1900-0AB71-0RG0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: release",87.5,"ST",100,"CP",8.0000000000000004E-4,10,"3SU19000AB710RG0"]
["3SU1900-0AB71-0RH0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: brake",87.5,"ST",100,"CP",1E-3,10,"3SU19000AB710RH0"]
["3SU1900-0AB71-0RJ0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: brake release",87.5,"ST",100,"CP",2E-3,10,"3SU19000AB710RJ0"]
["3SU1900-0AB71-0RK0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: lock",87.5,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AB710RK0"]
["3SU1900-0AB71-0RL0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: unlock",87.5,"ST",100,"CP",4.0000000000000001E-3,10,"3SU19000AB710RL0"]
["3SU1900-0AB71-0RM0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: set up",87.5,"ST",100,"CP",1.4E-2,10,"3SU19000AB710RM0"]
["3SU1900-0AB71-0RN0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: on/off momentary contact",87.5,"ST",100,"CP",3.8999999999999999E-4,10,"3SU19000AB710RN0"]
["3SU1900-0AB71-0RP0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: manual operation",87.5,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AB710RP0"]
["3SU1900-0AB71-0RQ0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: automatic sequence",87.5,"ST",100,"CP",3.8999999999999999E-4,10,"3SU19000AB710RQ0"]
["3SU1900-0AB71-0RR0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: suction",87.5,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AB710RR0"]
["3SU1900-0AB71-0RS0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: blow",87.5,"ST",100,"CP",5.0000000000000001E-3,10,"3SU19000AB710RS0"]
["3SU1900-0AC16-0AA0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, without inscription, for self-labeling",42.1,"ST",100,"CP",5.2999999999999998E-4,10,"3SU19000AC160AA0"]
["3SU1900-0AC16-0AB0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: On",68.899999999999991,"ST",100,"CP",5.9999999999999995E-4,10,"3SU19000AC160AB0"]
["3SU1900-0AC16-0AC0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Off",68.899999999999991,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AC160AC0"]
["3SU1900-0AC16-0AD0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Up",68.899999999999991,"ST",100,"CP",3.0000000000000001E-3,10,"3SU19000AC160AD0"]
["3SU1900-0AC16-0AE0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Down",68.899999999999991,"ST",100,"CP",2E-3,10,"3SU19000AC160AE0"]
["3SU1900-0AC16-0AF0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Forward",57.2,"ST",100,"CP",2E-3,10,"3SU19000AC160AF0"]
["3SU1900-0AC16-0AG0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Back",68.899999999999991,"ST",100,"CP",4.0000000000000001E-3,10,"3SU19000AC160AG0"]
["3SU1900-0AC16-0AH0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Right",68.899999999999991,"ST",100,"CP",2E-3,10,"3SU19000AC160AH0"]
["3SU1900-0AC16-0AJ0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Left",68.899999999999991,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AC160AJ0"]
["3SU1900-0AC16-0AK0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Stop",68.899999999999991,"ST",100,"CP",1E-3,10,"3SU19000AC160AK0"]
["3SU1900-0AC16-0AL0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Close",68.899999999999991,"ST",100,"CP",8.0000000000000004E-4,10,"3SU19000AC160AL0"]
["3SU1900-0AC16-0AP0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: operation",68.899999999999991,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AC160AP0"]
["3SU1900-0AC16-0AQ0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Fault",68.899999999999991,"ST",100,"CP",4.9700000000000005E-4,10,"3SU19000AC160AQ0"]
["3SU1900-0AC16-0DB0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Manual Auto",68.899999999999991,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AC160DB0"]
["3SU1900-0AC16-0DC0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Stop Start",68.899999999999991,"ST",100,"CP",6.6700000000000006E-4,10,"3SU19000AC160DC0"]
["3SU1900-0AC16-0DD0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Manual O Auto",68.899999999999991,"ST",100,"CP",5.1900000000000004E-4,10,"3SU19000AC160DD0"]
["3SU1900-0AC16-0DE0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Jog",68.899999999999991,"ST",100,"CP",1.0000000000000001E-5,10,"3SU19000AC160DE0"]
["3SU1900-0AC16-0DF0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Power Off",68.899999999999991,"ST",100,"CP",3.0000000000000001E-3,10,"3SU19000AC160DF0"]
["3SU1900-0AC16-0DG0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Power On",57.2,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AC160DG0"]
["3SU1900-0AC16-0DH0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Off On",68.899999999999991,"ST",100,"CP",8.0000000000000004E-4,10,"3SU19000AC160DH0"]
["3SU1900-0AC16-0DJ0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: On",57.2,"ST",100,"CP",4.0000000000000001E-3,10,"3SU19000AC160DJ0"]
["3SU1900-0AC16-0DK0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Off",57.2,"ST",100,"CP",4.0000000000000001E-3,10,"3SU19000AC160DK0"]
["3SU1900-0AC16-0DL0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Up",68.899999999999991,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AC160DL0"]
["3SU1900-0AC16-0DM0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Down",68.899999999999991,"ST",100,"CP",5.0000000000000001E-3,10,"3SU19000AC160DM0"]
["3SU1900-0AC16-0DN0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: forward",68.899999999999991,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AC160DN0"]
["3SU1900-0AC16-0DP0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Reverse",68.899999999999991,"ST",100,"CP",1E-3,10,"3SU19000AC160DP0"]
["3SU1900-0AC16-0DQ0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Right",68.899999999999991,"ST",100,"CP",9.9500000000000001E-4,10,"3SU19000AC160DQ0"]
["3SU1900-0AC16-0DR0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: left",68.899999999999991,"ST",100,"CP",2E-3,10,"3SU19000AC160DR0"]
["3SU1900-0AC16-0DS0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Stop",57.2,"ST",100,"CP",2E-3,10,"3SU19000AC160DS0"]
["3SU1900-0AC16-0DT0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: start",57.2,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AC160DT0"]
["3SU1900-0AC16-0DU0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Reset",57.2,"ST",100,"CP",4.0000000000000002E-4,10,"3SU19000AC160DU0"]
["3SU1900-0AC16-0DV0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: test",68.899999999999991,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AC160DV0"]
["3SU1900-0AC16-0DW0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Open",68.899999999999991,"ST",100,"CP",1E-3,10,"3SU19000AC160DW0"]
["3SU1900-0AC16-0DX0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Close",68.899999999999991,"ST",100,"CP",4.0000000000000001E-3,10,"3SU19000AC160DX0"]
["3SU1900-0AC16-0DY0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Manual O Auto",57.2,"ST",100,"CP",7.2999999999999996E-4,10,"3SU19000AC160DY0"]
["3SU1900-0AC16-0EA0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Manual Auto",57.2,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AC160EA0"]
["3SU1900-0AC16-0EB0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Running",68.899999999999991,"ST",100,"CP",2E-3,10,"3SU19000AC160EB0"]
["3SU1900-0AC16-0EC0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Fault",68.899999999999991,"ST",100,"CP",5.9899999999999992E-4,10,"3SU19000AC160EC0"]
["3SU1900-0AC16-0ED0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Run",68.899999999999991,"ST",100,"CP",4.0000000000000001E-3,10,"3SU19000AC160ED0"]
["3SU1900-0AC16-0GA0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Marche",68.899999999999991,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AC160GA0"]
["3SU1900-0AC16-0GB0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Arret",68.899999999999991,"ST",100,"CP",3.3E-4,10,"3SU19000AC160GB0"]
["3SU1900-0AC16-0GC0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Montee",68.899999999999991,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AC160GC0"]
["3SU1900-0AC16-0GD0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: descente",68.899999999999991,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AC160GD0"]
["3SU1900-0AC16-0GE0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Avant",68.899999999999991,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AC160GE0"]
["3SU1900-0AC16-0GF0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Retour",68.899999999999991,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AC160GF0"]
["3SU1900-0AC16-0GG0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Droite",68.899999999999991,"ST",100,"CP",2E-3,10,"3SU19000AC160GG0"]
["3SU1900-0AC16-0GH0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Gauche",68.899999999999991,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AC160GH0"]
["3SU1900-0AC16-0GJ0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Ouvert",68.899999999999991,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AC160GJ0"]
["3SU1900-0AC16-0GK0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Ferme",68.899999999999991,"ST",100,"CP",1E-3,10,"3SU19000AC160GK0"]
["3SU1900-0AC16-0GL0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Rapide",68.899999999999991,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AC160GL0"]
["3SU1900-0AC16-0GM0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: En Service",68.899999999999991,"ST",100,"CP",2E-3,10,"3SU19000AC160GM0"]
["3SU1900-0AC16-0GN0","Labeling plate for snapping on or gluing on label holder, label size 12.5x27 mm, black label, white font, with inscription: DΓ©faut",68.899999999999991,"ST",100,"CP",5.9999999999999995E-4,10,"3SU19000AC160GN0"]
["3SU1900-0AC16-0GP0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Reglage",68.899999999999991,"ST",100,"CP",1E-3,10,"3SU19000AC160GP0"]
["3SU1900-0AC16-0GQ0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: ArrΓt d'urgence",68.899999999999991,"ST",100,"CP",8.8000000000000003E-4,10,"3SU19000AC160GQ0"]
["3SU1900-0AC16-0GR0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Hors service",68.899999999999991,"ST",100,"CP",1E-3,10,"3SU19000AC160GR0"]
["3SU1900-0AC16-0GS0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Sous tension",68.899999999999991,"ST",100,"CP",3.8999999999999999E-4,10,"3SU19000AC160GS0"]
["3SU1900-0AC16-0GT0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Manu Auto",68.899999999999991,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AC160GT0"]
["3SU1900-0AC16-0GU0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Marche ArrΓt",68.899999999999991,"ST",100,"CP",8.0000000000000004E-4,10,"3SU19000AC160GU0"]
["3SU1900-0AC16-0GV0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with inscription: Rearmement",68.899999999999991,"ST",100,"CP",5.9899999999999992E-4,10,"3SU19000AC160GV0"]
["3SU1900-0AC16-0QA0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with graphic symbol: O",57.2,"ST",100,"CP",1E-3,10,"3SU19000AC160QA0"]
["3SU1900-0AC16-0QB0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with graphic symbol: I",57.2,"ST",100,"CP",1E-3,10,"3SU19000AC160QB0"]
["3SU1900-0AC16-0QG0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with graphic symbol: O  I",57.2,"ST",100,"CP",5.2000000000000006E-4,10,"3SU19000AC160QG0"]
["3SU1900-0AC16-0QJ0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with graphic symbol: 1  2",68.899999999999991,"ST",100,"CP",3.0000000000000001E-3,10,"3SU19000AC160QJ0"]
["3SU1900-0AC16-0QS0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, black label, white font, with graphic symbol:",68.899999999999991,"ST",100,"CP",4.28E-4,10,"3SU19000AC160QS0"]
["3SU1900-0AC81-0AA0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, without inscription, for self-labeling",61,"ST",100,"CP",5.4000000000000001E-4,10,"3SU19000AC810AA0"]
["3SU1900-0AC81-0AB0","Labeling plate for snapping on or adhering to label holder, label size 12.5x27 mm, silver label, black font, with inscription: On",87.5,"ST",100,"CP",5.8999999999999992E-4,10,"3SU19000AC810AB0"]
["3SU1900-0AC81-0AC0","Labeling plate for snapping on or adhering to label holder, label size 12.5x27 mm, silver label, black font, with inscription: Off",87.5,"ST",100,"CP",5.9999999999999995E-4,10,"3SU19000AC810AC0"]
["3SU1900-0AC81-0AD0","Labeling plate for snapping on or adhering to label holder, label size 12.5x27 mm, silver label, black font, with inscription: Up",87.5,"ST",100,"CP",8.0000000000000004E-4,10,"3SU19000AC810AD0"]
["3SU1900-0AC81-0AE0","Labeling plate for snapping on or adhering to label holder, label size 12.5x27 mm, silver label, black font, with inscription: Down",87.5,"ST",100,"CP",1E-3,10,"3SU19000AC810AE0"]
["3SU1900-0AC81-0AF0","Labeling plate for snapping on or adhering to label holder, label size 12.5x27 mm, silver label, black font, with inscription: In front",87.5,"ST",100,"CP",1E-3,10,"3SU19000AC810AF0"]
["3SU1900-0AC81-0AG0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with inscription: Back",87.5,"ST",100,"CP",4.0000000000000001E-3,10,"3SU19000AC810AG0"]
["3SU1900-0AC81-0AH0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with inscription: Right",87.5,"ST",100,"CP",2E-3,10,"3SU19000AC810AH0"]
["3SU1900-0AC81-0AJ0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with inscription: Left",87.5,"ST",100,"CP",2E-3,10,"3SU19000AC810AJ0"]
["3SU1900-0AC81-0AK0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with inscription: Stop",87.5,"ST",100,"CP",3.0000000000000001E-3,10,"3SU19000AC810AK0"]
["3SU1900-0AC81-0AL0","Labeling plate for snapping on or adhering to label holder, label size 12.5x27 mm, silver label, black font, with inscription: Closed",87.5,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AC810AL0"]
["3SU1900-0AC81-0AM0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with inscription: fast",87.5,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AC810AM0"]
["3SU1900-0AC81-0AN0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with inscription: slow",87.5,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AC810AN0"]
["3SU1900-0AC81-0AP0","Labeling plate for snapping on or adhering to label holder, label size 12.5x27 mm, silver label, black font, with inscription: Operation",87.5,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AC810AP0"]
["3SU1900-0AC81-0AQ0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with inscription: Fault",87.5,"ST",100,"CP",5.8999999999999992E-4,10,"3SU19000AC810AQ0"]
["3SU1900-0AC81-0AR0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with inscription: set-up",87.5,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AC810AR0"]
["3SU1900-0AC81-0DB0","Labeling plate for snapping on or adhering to label holder, label size 12.5x27 mm, silver label, black font, with inscription: Manual Auto",87.5,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AC810DB0"]
["3SU1900-0AC81-0DC0","Labeling plate for snapping on or adhering to label holder, label size 12.5x27 mm, silver label, black font, with inscription: Stop Start",87.5,"ST",100,"CP",2E-3,10,"3SU19000AC810DC0"]
["3SU1900-0AC81-0DD0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with inscription: Manual O Auto",87.5,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AC810DD0"]
["3SU1900-0AC81-0DJ0","Labeling plate for snapping on or adhering to label holder, label size 12.5x27 mm, silver label, black font, with inscription: On",87.5,"ST",100,"CP",3.6299999999999999E-4,10,"3SU19000AC810DJ0"]
["3SU1900-0AC81-0DK0","Labeling plate for snapping on or adhering to label holder, label size 12.5x27 mm, silver label, black font, with inscription: Off",87.5,"ST",100,"CP",2E-3,10,"3SU19000AC810DK0"]
["3SU1900-0AC81-0DL0","Labeling plate for snapping on or adhering to label holder, label size 12.5x27 mm, silver label, black font, with inscription: Up",87.5,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AC810DL0"]
["3SU1900-0AC81-0DM0","Labeling plate for snapping on or adhering to label holder, label size 12.5x27 mm, silver label, black font, with inscription: Down",87.5,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AC810DM0"]
["3SU1900-0AC81-0DS0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with inscription:",87.5,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AC810DS0"]
["3SU1900-0AC81-0DT0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with inscription: start",87.5,"ST",100,"CP",3.9899999999999999E-4,10,"3SU19000AC810DT0"]
["3SU1900-0AC81-0DU0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with inscription: Reset",87.5,"ST",100,"CP",5.8999999999999992E-4,10,"3SU19000AC810DU0"]
["3SU1900-0AC81-0DV0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with inscription: test",87.5,"ST",100,"CP",2E-3,10,"3SU19000AC810DV0"]
["3SU1900-0AC81-0DW0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with inscription: Open",87.5,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AC810DW0"]
["3SU1900-0AC81-0DX0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with inscription: Close",87.5,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AC810DX0"]
["3SU1900-0AC81-0DY0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with inscription: Manual O Auto",80,"ST",100,"CP",8.0000000000000004E-4,10,"3SU19000AC810DY0"]
["3SU1900-0AC81-0EA0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with inscription: Manual Auto",87.5,"ST",100,"CP",8.0000000000000004E-4,10,"3SU19000AC810EA0"]
["3SU1900-0AC81-0EB0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with inscription: Running",87.5,"ST",100,"CP",3.6999999999999999E-4,10,"3SU19000AC810EB0"]
["3SU1900-0AC81-0EC0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with inscription: Fault",87.5,"ST",100,"CP",8.0000000000000004E-4,10,"3SU19000AC810EC0"]
["3SU1900-0AC81-0EE0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with inscription: Fast",87.5,"ST",100,"CP",2E-3,10,"3SU19000AC810EE0"]
["3SU1900-0AC81-0EF0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with inscription: Slow",87.5,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AC810EF0"]
["3SU1900-0AC81-0QA0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with graphic symbol:",87.5,"ST",100,"CP",3.0000000000000001E-3,10,"3SU19000AC810QA0"]
["3SU1900-0AC81-0QB0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with graphic symbol: I",87.5,"ST",100,"CP",8.0000000000000004E-4,10,"3SU19000AC810QB0"]
["3SU1900-0AC81-0QC0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with graphic symbol: II",87.5,"ST",100,"CP",8.0000000000000004E-4,10,"3SU19000AC810QC0"]
["3SU1900-0AC81-0QD0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with graphic symbol: III",87.5,"ST",100,"CP",1E-3,10,"3SU19000AC810QD0"]
["3SU1900-0AC81-0QG0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with graphic symbol: O I",80,"ST",100,"CP",8.4999999999999995E-4,10,"3SU19000AC810QG0"]
["3SU1900-0AC81-0QK0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with graphic symbol: I O II",80,"ST",100,"CP",5.9999999999999995E-4,10,"3SU19000AC810QK0"]
["3SU1900-0AC81-0QL0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with graphic symbol: 1 O 2",74.5,"ST",100,"CP",1E-3,10,"3SU19000AC810QL0"]
["3SU1900-0AC81-0QR0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with graphic symbol: arrow pointing to the right",87.5,"ST",100,"CP",6.9999999999999999E-4,10,"3SU19000AC810QR0"]
["3SU1900-0AC81-0QS0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with graphic symbol: arrow pointing up",87.5,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AC810QS0"]
["3SU1900-0AD16-0AA0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, without inscription, for self-labeling",42.1,"ST",100,"CP",6.8000000000000005E-4,10,"3SU19000AD160AA0"]
["3SU1900-0AD16-0AB0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: On",68.899999999999991,"ST",100,"CP",4.0000000000000001E-3,10,"3SU19000AD160AB0"]
["3SU1900-0AD16-0AC0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Off",68.899999999999991,"ST",100,"CP",1E-3,10,"3SU19000AD160AC0"]
["3SU1900-0AD16-0AD0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Up",68.899999999999991,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AD160AD0"]
["3SU1900-0AD16-0AE0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Down",68.899999999999991,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AD160AE0"]
["3SU1900-0AD16-0AF0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Forward",68.899999999999991,"ST",100,"CP",1E-3,10,"3SU19000AD160AF0"]
["3SU1900-0AD16-0AG0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Back",68.899999999999991,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AD160AG0"]
["3SU1900-0AD16-0AK0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Stop",68.899999999999991,"ST",100,"CP",1E-3,10,"3SU19000AD160AK0"]
["3SU1900-0AD16-0AL0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Close",68.899999999999991,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AD160AL0"]
["3SU1900-0AD16-0AP0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: operation",68.899999999999991,"ST",100,"CP",1E-3,10,"3SU19000AD160AP0"]
["3SU1900-0AD16-0AQ0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Fault",68.899999999999991,"ST",100,"CP",5.9999999999999995E-4,10,"3SU19000AD160AQ0"]
["3SU1900-0AD16-0DB0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Manual Auto",68.899999999999991,"ST",100,"CP",5.9899999999999992E-4,10,"3SU19000AD160DB0"]
["3SU1900-0AD16-0DC0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Stop Start",68.899999999999991,"ST",100,"CP",2E-3,10,"3SU19000AD160DC0"]
["3SU1900-0AD16-0DJ0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: On",57.2,"ST",100,"CP",6.9999999999999999E-4,10,"3SU19000AD160DJ0"]
["3SU1900-0AD16-0DK0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Off",57.2,"ST",100,"CP",5.9999999999999995E-4,10,"3SU19000AD160DK0"]
["3SU1900-0AD16-0DL0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Up",68.899999999999991,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AD160DL0"]
["3SU1900-0AD16-0DM0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Down",68.899999999999991,"ST",100,"CP",5.0000000000000002E-5,10,"3SU19000AD160DM0"]
["3SU1900-0AD16-0DN0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Forward",68.899999999999991,"ST",100,"CP",3.0000000000000001E-3,10,"3SU19000AD160DN0"]
["3SU1900-0AD16-0DP0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Reverse",68.899999999999991,"ST",100,"CP",4.0000000000000001E-3,10,"3SU19000AD160DP0"]
["3SU1900-0AD16-0DQ0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Right",68.899999999999991,"ST",100,"CP",2E-3,10,"3SU19000AD160DQ0"]
["3SU1900-0AD16-0DS0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Stop",60,"ST",100,"CP",7.1400000000000001E-4,10,"3SU19000AD160DS0"]
["3SU1900-0AD16-0DT0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: start",60,"ST",100,"CP",4.0000000000000001E-3,10,"3SU19000AD160DT0"]
["3SU1900-0AD16-0DW0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Open",57.2,"ST",100,"CP",9.9500000000000001E-4,10,"3SU19000AD160DW0"]
["3SU1900-0AD16-0DX0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Close",57.2,"ST",100,"CP",1E-3,10,"3SU19000AD160DX0"]
["3SU1900-0AD16-0EA0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Manual Auto",60,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AD160EA0"]
["3SU1900-0AD16-0EB0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Running",60,"ST",100,"CP",5.9999999999999995E-4,10,"3SU19000AD160EB0"]
["3SU1900-0AD16-0EC0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Fault",60,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AD160EC0"]
["3SU1900-0AD16-0GA0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Marche",68.899999999999991,"ST",100,"CP",1E-3,10,"3SU19000AD160GA0"]
["3SU1900-0AD16-0GB0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Arret",68.899999999999991,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AD160GB0"]
["3SU1900-0AD16-0GG0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Droite",68.899999999999991,"ST",100,"CP",2E-3,10,"3SU19000AD160GG0"]
["3SU1900-0AD16-0GH0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Gauche",68.899999999999991,"ST",100,"CP",2E-3,10,"3SU19000AD160GH0"]
["3SU1900-0AD16-0GM0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: En Service",68.899999999999991,"ST",100,"CP",6.0000000000000001E-3,10,"3SU19000AD160GM0"]
["3SU1900-0AD16-0GN0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Defaut",68.899999999999991,"ST",100,"CP",3.0000000000000001E-3,10,"3SU19000AD160GN0"]
["3SU1900-0AD16-0GS0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Sous Tension",68.899999999999991,"ST",100,"CP",2E-3,10,"3SU19000AD160GS0"]
["3SU1900-0AD16-0GT0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Manu Auto",68.899999999999991,"ST",100,"CP",1E-3,10,"3SU19000AD160GT0"]
["3SU1900-0AD16-0GU0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Marche ArrΓt",68.899999999999991,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AD160GU0"]
["3SU1900-0AD16-0GV0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with inscription: Rearmement",68.899999999999991,"ST",100,"CP",4.0000000000000001E-3,10,"3SU19000AD160GV0"]
["3SU1900-0AD16-0QA0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with graphic symbol: O",60,"ST",100,"CP",7.9799999999999999E-4,10,"3SU19000AD160QA0"]
["3SU1900-0AD16-0QB0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with graphic symbol: I",60,"ST",100,"CP",1E-3,10,"3SU19000AD160QB0"]
["3SU1900-0AD16-0QG0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with graphic symbol: O I",60,"ST",100,"CP",8.0000000000000004E-4,10,"3SU19000AD160QG0"]
["3SU1900-0AD16-0QR0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with graphic symbol: arrow pointing to the right",68.899999999999991,"ST",100,"CP",5.9999999999999995E-4,10,"3SU19000AD160QR0"]
["3SU1900-0AD16-0QS0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, black label, white font, with graphic symbol: arrow pointing up",68.899999999999991,"ST",100,"CP",5.9999999999999995E-4,10,"3SU19000AD160QS0"]
["3SU1900-0AD70-0AA0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, transparent, without inscription, for self-labeling",68.899999999999991,"ST",100,"CP",6.9999999999999999E-4,10,"3SU19000AD700AA0"]
["3SU1900-0AD81-0AA0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, without inscription, for self-labeling",61,"ST",100,"CP",6.4000000000000005E-4,10,"3SU19000AD810AA0"]
["3SU1900-0AD81-0AB0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with inscription: On",87.5,"ST",100,"CP",6.6300000000000007E-4,10,"3SU19000AD810AB0"]
["3SU1900-0AD81-0AC0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with inscription: Off",87.5,"ST",100,"CP",2E-3,10,"3SU19000AD810AC0"]
["3SU1900-0AD81-0AD0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with inscription: Up",87.5,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AD810AD0"]
["3SU1900-0AD81-0AE0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with inscription: Down",87.5,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AD810AE0"]
["3SU1900-0AD81-0AF0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with inscription: Forward",87.5,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AD810AF0"]
["3SU1900-0AD81-0AG0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with inscription: Back",87.5,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AD810AG0"]
["3SU1900-0AD81-0AH0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with inscription: Right",87.5,"ST",100,"CP",1E-3,10,"3SU19000AD810AH0"]
["3SU1900-0AD81-0AK0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with inscription: Stop",87.5,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AD810AK0"]
["3SU1900-0AD81-0AL0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with inscription: Close",87.5,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AD810AL0"]
["3SU1900-0AD81-0AP0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with inscription: operation",87.5,"ST",100,"CP",8.0000000000000004E-4,10,"3SU19000AD810AP0"]
["3SU1900-0AD81-0AQ0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with inscription: Fault",87.5,"ST",100,"CP",1E-3,10,"3SU19000AD810AQ0"]
["3SU1900-0AD81-0DB0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with inscription: Manual Auto",87.5,"ST",100,"CP",8.0000000000000004E-4,10,"3SU19000AD810DB0"]
["3SU1900-0AD81-0DD0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with inscription: Manual O Auto",87.5,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AD810DD0"]
["3SU1900-0AD81-0DJ0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with inscription: On",87.5,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AD810DJ0"]
["3SU1900-0AD81-0DK0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with inscription: Off",87.5,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AD810DK0"]
["3SU1900-0AD81-0DS0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with inscription: Stop",87.5,"ST",100,"CP",1E-3,10,"3SU19000AD810DS0"]
["3SU1900-0AD81-0DT0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with inscription: start",87.5,"ST",100,"CP",8.0000000000000004E-4,10,"3SU19000AD810DT0"]
["3SU1900-0AD81-0DU0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with inscription: Reset",87.5,"ST",100,"CP",5.9999999999999995E-4,10,"3SU19000AD810DU0"]
["3SU1900-0AD81-0DY0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with inscription: Manual O Auto",87.5,"ST",100,"CP",1E-3,10,"3SU19000AD810DY0"]
["3SU1900-0AD81-0EC0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with inscription: Fault",87.5,"ST",100,"CP",4.0000000000000001E-3,10,"3SU19000AD810EC0"]
["3SU1900-0AD81-0QA0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with graphic symbol: O",87.5,"ST",100,"CP",1E-3,10,"3SU19000AD810QA0"]
["3SU1900-0AD81-0QB0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with graphic symbol: I",87.5,"ST",100,"CP",2E-3,10,"3SU19000AD810QB0"]
["3SU1900-0AD81-0QG0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with graphic symbol: O I",87.5,"ST",100,"CP",6.6300000000000007E-4,10,"3SU19000AD810QG0"]
["3SU1900-0AD81-0QK0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with graphic symbol: I O II",87.5,"ST",100,"CP",1E-3,10,"3SU19000AD810QK0"]
["3SU1900-0AD81-0QL0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with graphic symbol: 1 O 2",87.5,"ST",100,"CP",1E-3,10,"3SU19000AD810QL0"]
["3SU1900-0AD81-0QR0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with graphic symbol: arrow pointing to the right",87.5,"ST",100,"CP",6.8000000000000005E-4,10,"3SU19000AD810QR0"]
["3SU1900-0AD81-0QS0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with graphic symbol: arrow pointing up",87.5,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AD810QS0"]
["3SU1900-0AE16-0AA0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, without inscription, for self-labeling",60,"ST",100,"CP",9.1E-4,10,"3SU19000AE160AA0"]
["3SU1900-0AE16-0AB0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: On",76.399999999999991,"ST",100,"CP",4.0000000000000001E-3,10,"3SU19000AE160AB0"]
["3SU1900-0AE16-0AC0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Off",76.399999999999991,"ST",100,"CP",4.0000000000000001E-3,10,"3SU19000AE160AC0"]
["3SU1900-0AE16-0AD0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Up",76.399999999999991,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AE160AD0"]
["3SU1900-0AE16-0AE0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Down",76.399999999999991,"ST",100,"CP",1E-3,10,"3SU19000AE160AE0"]
["3SU1900-0AE16-0AF0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Forward",76.399999999999991,"ST",100,"CP",8.9999999999999998E-4,10,"3SU19000AE160AF0"]
["3SU1900-0AE16-0AG0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Back",76.399999999999991,"ST",100,"CP",1E-3,10,"3SU19000AE160AG0"]
["3SU1900-0AE16-0AH0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Right",76.399999999999991,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AE160AH0"]
["3SU1900-0AE16-0AJ0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Left",76.399999999999991,"ST",100,"CP",1E-3,10,"3SU19000AE160AJ0"]
["3SU1900-0AE16-0AK0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Stop",76.399999999999991,"ST",100,"CP",1E-3,10,"3SU19000AE160AK0"]
["3SU1900-0AE16-0AL0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Close",76.399999999999991,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AE160AL0"]
["3SU1900-0AE16-0AP0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: operation",76.399999999999991,"ST",100,"CP",1E-3,10,"3SU19000AE160AP0"]
["3SU1900-0AE16-0AQ0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Fault",76.399999999999991,"ST",100,"CP",4.0000000000000001E-3,10,"3SU19000AE160AQ0"]
["3SU1900-0AE16-0DA0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: EMERGENCY STOP",76.399999999999991,"ST",100,"CP",2E-3,10,"3SU19000AE160DA0"]
["3SU1900-0AE16-0DB0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Manual Auto",76.399999999999991,"ST",100,"CP",2E-3,10,"3SU19000AE160DB0"]
["3SU1900-0AE16-0DC0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Stop Start",76.399999999999991,"ST",100,"CP",1E-3,10,"3SU19000AE160DC0"]
["3SU1900-0AE16-0DJ0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: On",70,"ST",100,"CP",2E-3,10,"3SU19000AE160DJ0"]
["3SU1900-0AE16-0DK0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Off",70,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AE160DK0"]
["3SU1900-0AE16-0DL0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Up",76.399999999999991,"ST",100,"CP",1E-3,10,"3SU19000AE160DL0"]
["3SU1900-0AE16-0DM0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Down",76.399999999999991,"ST",100,"CP",8.9999999999999998E-4,10,"3SU19000AE160DM0"]
["3SU1900-0AE16-0DN0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Forward",76.399999999999991,"ST",100,"CP",3.0000000000000001E-3,10,"3SU19000AE160DN0"]
["3SU1900-0AE16-0DP0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Reverse",76.399999999999991,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AE160DP0"]
["3SU1900-0AE16-0DS0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Stop",70,"ST",100,"CP",1.0000000000000001E-5,10,"3SU19000AE160DS0"]
["3SU1900-0AE16-0DT0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: start",70,"ST",100,"CP",9.9999999999999995E-7,10,"3SU19000AE160DT0"]
["3SU1900-0AE16-0GA0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Marche",76.399999999999991,"ST",100,"CP",6.9999999999999999E-4,10,"3SU19000AE160GA0"]
["3SU1900-0AE16-0GB0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Arret",76.399999999999991,"ST",100,"CP",4.0000000000000001E-3,10,"3SU19000AE160GB0"]
["3SU1900-0AE16-0GC0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Montee",76.399999999999991,"ST",100,"CP",9.9500000000000001E-4,10,"3SU19000AE160GC0"]
["3SU1900-0AE16-0GD0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Descente",76.399999999999991,"ST",100,"CP",9.9500000000000001E-4,10,"3SU19000AE160GD0"]
["3SU1900-0AE16-0GM0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: En Service",76.399999999999991,"ST",100,"CP",2E-3,10,"3SU19000AE160GM0"]
["3SU1900-0AE16-0GN0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Defaut",76.399999999999991,"ST",100,"CP",1E-3,10,"3SU19000AE160GN0"]
["3SU1900-0AE16-0GS0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Sous tension",76.399999999999991,"ST",100,"CP",1E-3,10,"3SU19000AE160GS0"]
["3SU1900-0AE16-0GT0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Manu Auto",76.399999999999991,"ST",100,"CP",5.0000000000000001E-4,10,"3SU19000AE160GT0"]
["3SU1900-0AE16-0GU0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with inscription: Marche ArrΓt",76.399999999999991,"ST",100,"CP",8.0000000000000004E-4,10,"3SU19000AE160GU0"]
["3SU1900-0AE16-0QG0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with graphic symbol: O  I",70,"ST",100,"CP",2E-3,10,"3SU19000AE160QG0"]
["3SU1900-0AE16-0QR0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, black label, white font, with graphic symbol: arrow pointing to the right",76.399999999999991,"ST",100,"CP",8.5999999999999998E-4,10,"3SU19000AE160QR0"]
["3SU1900-0AE81-0AA0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, silver label, black font, without inscription, for self-labeling",80.399999999999991,"ST",100,"CP",9.2299999999999999E-4,10,"3SU19000AE810AA0"]
["3SU1900-0AF16-0AA0","Labeling plate for gluing on enclosure, label size 22x22 mm, black label, white font, without inscription, for self-labeling",63.800000000000004,"ST",100,"CP",6.8000000000000005E-4,10,"3SU19000AF160AA0"]
["3SU1900-0AF81-0AA0","Labeling plate for gluing on enclosure, label size 22x22mm, silver label, black font, without inscription, for self-labeling",80.399999999999991,"ST",100,"CP",6.8000000000000005E-4,10,"3SU19000AF810AA0"]
["3SU1900-0AG10-0AA0","Label holder, 22mm, flat, Frame rounded off at the bottom black, for labeling plate 12.5 mm x 27 mm, for gluing",60,"ST",100,"CP",2E-3,10,"3SU19000AG100AA0"]
["3SU1900-0AH10-0AA0","Label holder, 22mm, flat, Frame rounded off at the bottom black, for labeling plate 17.5 mm x 27 mm, for gluing",60,"ST",100,"CP",2E-3,10,"3SU19000AH100AA0"]
["3SU1900-0AJ10-0AA0","Label holder, 22mm, flat, Frame rounded off at the bottom black, for labeling plate 27mm x 27mm, for gluing",60,"ST",100,"CP",3.0000000000000001E-3,10,"3SU19000AJ100AA0"]
["3SU1900-0AK10-0AA0","Label holder, 22mm, for twin pushbutton, flat, black, for labeling plate 12.5 mm x 27 mm",60.1,"ST",100,"CP",3.0000000000000001E-3,10,"3SU19000AK100AA0"]
["3SU1900-0AN10-0AA0","Label holder, 22mm, frame rectangular at the bottom, black, for labeling plate 12.5 mm x 27 mm, for gluing",60,"ST",100,"CP",2E-3,10,"3SU19000AN100AA0"]
["3SU1900-0AP10-0AA0","Label holder, 22mm, frame rectangular at the bottom, black, for labeling plate 17.5 mm x 27 mm, for gluing",60,"ST",100,"CP",3.0000000000000001E-3,10,"3SU19000AP100AA0"]
["3SU1900-0AQ10-0AA0","Label holder, 22mm, frame rectangular at the bottom, black, for labeling plate 27mm x 27mm, for gluing",60,"ST",100,"CP",3.0000000000000001E-3,10,"3SU19000AQ100AA0"]
["3SU1900-0AR10-0AA0","Label holder, 22mm, flat, Frame rounded off at the bottom black, for labeling plate 12.5 mm x 27 mm, for snapping on",60,"ST",100,"CP",2E-3,10,"3SU19000AR100AA0"]
["3SU1900-0AS10-0AA0","Label holder, 22mm, flat, Frame rounded off at the bottom black, for labeling plate 17.5 mm x 27 mm, for snapping on",60,"ST",100,"CP",2E-3,10,"3SU19000AS100AA0"]
["3SU1900-0AT10-0AA0","Label holder, 22mm, flat, Frame rounded off at the bottom black, for labeling plate 27mm x 27mm, for snapping on",60,"ST",100,"CP",2E-3,10,"3SU19000AT100AA0"]
["3SU1900-0AY61-0AA0","Unit labeling plate, white, without inscription, for support of dust resistance, for contact modules",50,"ST",100,"CP",2.3999999999999998E-4,10,"3SU19000AY610AA0"]
["3SU1900-0BH60-0AA0","Inscription plates for printing for illuminated pushbutton, milky, without inscription, for self-labeling, 7 sheets A4, 490 labels",43,"ST",100,"CP",2.61E-4,490,"3SU19000BH600AA0"]
["3SU1900-0BJ61-0AA0","Labeling plates for printing and gluing on label holder, label size 12.5x27mm, white, without inscription, for self-labeling, 5 sheets A4, 480 labels",37.4,"ST",100,"CP",1.9700000000000002E-4,480,"3SU19000BJ610AA0"]
["3SU1900-0BK61-0AA0","Labeling plates for printing and gluing on label holder, Label size 17.5 x 27 mm, white, without inscription, for self-labeling, 10 sheets A4, 720 labels",35.700000000000003,"ST",100,"CP",3.3800000000000003E-4,720,"3SU19000BK610AA0"]
["3SU1900-0BL61-0AA0","Labeling plates for printing and gluing on label holder, Label size 27x27 mm, white, without inscription, for self-labeling, 10 sheets A4, 480 labels",37.4,"ST",100,"CP",4.9899999999999999E-4,480,"3SU19000BL610AA0"]
["3SU1900-0BM61-0AA0","Labeling plates for printing and gluing on enclosure, label size 22x22 mm, white, without inscription, for self-labeling, 10 sheets A4, 700 labels",40,"ST",100,"CP",3.5E-4,700,"3SU19000BM610AA0"]
["3SU1900-0FT10-0AA0","pushbutton, flat, black, for pushbutton",68.899999999999991,"ST",100,"CP",8.0000000000000004E-4,10,"3SU19000FT100AA0"]
["3SU1900-0FT20-0AA0","pushbutton, flat, red, for pushbutton",68.899999999999991,"ST",100,"CP",5.9899999999999992E-4,10,"3SU19000FT200AA0"]
["3SU1900-0FT30-0AA0","pushbutton, flat, yellow, for pushbutton",68.899999999999991,"ST",100,"CP",1E-3,10,"3SU19000FT300AA0"]
["3SU1900-0FT40-0AA0","pushbutton, flat, green, for pushbutton",68.899999999999991,"ST",100,"CP",8.0000000000000004E-4,10,"3SU19000FT400AA0"]
["3SU1900-0FT50-0AA0","pushbutton, flat, blue, for pushbutton",68.899999999999991,"ST",100,"CP",6.6E-4,10,"3SU19000FT500AA0"]
["3SU1900-0FT60-0AA0","pushbutton, flat, white, for pushbutton",68.899999999999991,"ST",100,"CP",8.0000000000000004E-4,10,"3SU19000FT600AA0"]
["3SU1900-0KA10-0AA0","Printed circuit board holder, with screw, for mounting the command devices with the printed circuit board",62.9,"ST",100,"CP",6.0000000000000001E-3,10,"3SU19000KA100AA0"]
["3SU1900-0KC10-0AA0","Pressure piece for actuation of the center contact module of 3 contact modules, for selector switch, key-operated switch and twin pushbutton",40.300000000000004,"ST",100,"CP",3.2000000000000003E-4,10,"3SU19000KC100AA0"]
["3SU1901-0FT00-0AA0","pushbutton, flat, amber, for illuminated pushbutton",68.899999999999991,"ST",100,"CP",1E-3,10,"3SU19010FT000AA0"]
["3SU1901-0FT20-0AA0","pushbutton, flat, red, for illuminated pushbutton",68.899999999999991,"ST",100,"CP",8.0000000000000004E-4,10,"3SU19010FT200AA0"]
["3SU1901-0FT30-0AA0","pushbutton, flat, yellow, for illuminated pushbutton",68.899999999999991,"ST",100,"CP",5.9899999999999992E-4,10,"3SU19010FT300AA0"]
["3SU1901-0FT40-0AA0","pushbutton, flat, green, for illuminated pushbutton",68.899999999999991,"ST",100,"CP",8.0000000000000004E-4,10,"3SU19010FT400AA0"]
["3SU1901-0FT50-0AA0","pushbutton, flat, blue, for illuminated pushbutton",68.899999999999991,"ST",100,"CP",1E-3,10,"3SU19010FT500AA0"]
["3SU1901-0FT60-0AA0","pushbutton, flat, white, for illuminated pushbutton",68.899999999999991,"ST",100,"CP",6.9999999999999999E-4,10,"3SU19010FT600AA0"]
["3SU1901-0FT70-0AA0","pushbutton, flat, clear, for illuminated pushbutton",68.899999999999991,"ST",100,"CP",8.0000000000000004E-4,10,"3SU19010FT700AA0"]
["3SU1950-0KK80-0AA0","Grounding screw for metal bracket, grounding of metal actuators for installation in front plates made of non-conductive materials",10,"ST",100,"CP",5.0000000000000001E-4,50,"3SU19500KK800AA0"]
["3TX4210-0H","Unit labeling plate Pack with 100 blank labels loose, can be snapped on",20,"ST",100,"CP",1E-3,100,"3TX42100H"]
["3TX4210-0J","Pack with 100 label holders for mounting as required",11.799999999999999,"ST",100,"CP",2.8000000000000003E-4,100,"3TX42100J"]
["3TX4210-0R","Unit labeling plate can be snapped on consists of 380 labels",26.6,"ST",100,"CP",7.7800000000000005E-4,380,"3TX42100R"]
["3TX6426-0A","Adapter plate Sz. 1",77.899999999999991,"ST",100,"CP",4.2000000000000003E-2,10,"3TX64260A"]
["3TY6483-0BY80-0AH1","Magnet coil for contactors SPU 31V-48.5-52.5 ohm 2x 220 8 WD",8890,"ST",100,"CP",1.0760000000000001,1,"3TY64830BY800AH1"]
["3UF7925-0AA00-0","Labeling strips, for Operator panel 3UF720, for labeling the push-buttons",43.5,"ST",100,"CP",5.5000000000000003E-4,400,"3UF79250AA000"]
["3UF7925-0AA01-0","Labeling strips, for Operator panel with display 3UF721, for labeling the push-buttons",43.5,"ST",100,"CP",3.6600000000000001E-4,600,"3UF79250AA010"]
["3UF7925-0AA02-0","Labeling strips, for Operator panel 3UF720, for labeling the LED",29.8,"ST",100,"CP",1.8099999999999998E-4,1200,"3UF79250AA020"]
["3UX1017","Accessory for overload relay Holder for cable release",20.3,"ST",100,"CP",3.7999999999999999E-2,10,"3UX1017"]
["LZS:PT17021","Fixing/reject bracket for plug-in relay RT series and PT screw terminals logical and PT spring-loaded terminal socket logical disconnection",27.6,"ST",100,"CP",5.0000000000000001E-3,10,"LZS:PT17021"]
["LZS:PT17024","Fixing/reject bracket for plug-in relay RT series and PT screw terminal base not logical",30,"ST",100,"CP",4.0000000000000001E-3,10,"LZS:PT17024"]
["LZS:PT17040","Labeling plate 26 mm for PT relay",20,"ST",100,"CP",8.5999999999999998E-4,10,"LZS:PT17040"]
["LZS:RT17016","Fixing/reject bracket for plug-in relay RT series",50,"ST",100,"CP",3.0000000000000001E-3,10,"LZS:RT17016"]
["LZS:RT17040","Label 15 mm for RT and RY relay",20,"ST",100,"CP",6.0499999999999996E-4,10,"LZS:RT17040"]
["LZS:RT170P1","fanning strip 2-pole for RT push-in terminal sockets",71.099999999999994,"ST",100,"CP",1E-3,10,"LZS:RT170P1"]
["3RV1902-1AG6","Undervoltage release 100 V !!! Phased-out product !!! Successor is SIRIUS 3RV2","On request",null,null,"CP",0.13400000000000001,1,"3RV19021AG6"]
["3RV1922-1CU0","Undervoltage release 240 V AC, 50 Hz with leading auxiliary switch 2 NO, for circuit breaker Size S0...S3 !!! Phased-out product !!! Successor is SIRIUS 3RV2","On request",null,null,"CP",7.0000000000000001E-3,1,"3RV19221CU0"]
["3SB2901-2XZ",null,"on request",null,null,"CP",2E-3,0,"3SB29012XZ"]
["3SB2901-2XZ",null,"on request",null,null,"CP",2E-3,0,"3SB29012XZ"]
["3SU1803-0NZ00",null,"On Request",null,null,"CP",0.54300000000000004,0,"3SU18030NZ00"]
["3SU1900-0AD16-0AZ0",null,4,null,null,"CP",5.0000000000000001E-4,0,"3SU19000AD160AZ0"]
["3SU1900-0AD16-0AZ0",null,4,null,null,"CP",3.9E-2,0,"3SU19000AD160AZ0"]
["3SU1900-0AE16-0AZ0",null,4,null,null,"CP",1E-3,0,"3SU19000AE160AZ0"]
["3SU1900-0AF16-0AZ0",null,5.5,null,null,"CP",9.9999999999999995E-7,0,"3SU19000AF160AZ0"]
["LZS:PT5B7L24-A","Plug-in relay complete unit 4 W, 24 V DC LED module green Socket with logic isolation screw terminal 3.5 mm pinning",16.5,null,null,"CP",0.108,1,"LZS:PT5B7L24A"]
["LZS:RT3B6L24-A","Plug-in relay complete unit 1 W, 24 V DC LED module green Plug-in socket with safe isolation screw terminal",16.100000000000001,null,null,"CP",6.3E-2,1,"LZS:RT3B6L24A"]
["LZS:RT4B6L24-A","Plug-in relay complete unit 2 CO, 24 V DC LED module green Plug-in socket with logical separation, screw terminal",16.100000000000001,null,null,"CP",6.2E-2,1,"LZS:RT4B6L24A"]

{"sheet":"Sheet1","index":1,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["PA","PMD Data available"]
[""]
["VF","Sales Release"]
[""]
["LF","Delivery Release"]
[""]
["AE","Phase Out Announce"]
[""]
["TS","Prod. Cancellation"]
[""]
["MH","Prod. Discont."]
[""]
["AK","End Prod.Lifecycl."]