{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Price List 2020-2021","Sheet1"],"not_rendered":{"charts":0,"images":4,"macros":1,"external_links":0,"defined_names":3,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Price List 2020-2021","index":0,"n_rows":165337,"n_cols":8,"rows_kept":4500,"cut":true,"hidden":false,"merged":[[0,1,0,2],[0,3,0,6],[1,0,1,6],[2,2,2,6],[2,0,2,1]],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
[null,"Siemens Digital Industries\nΤιμοκατάλογος Προϊόντων Βιομηχανίας 2020-2021",null,"Ισχύει από την 01.11.2020 και καταργεί κάθε προηγούμενο. Οι τιμές και τα τεχνικά χαρακτηριστικά των υλικών υπόκεινται σε οποιαδήποτε αλλαγή χωρίς προηγούμενη ειδοποίηση και δεν περιλαμβάνουν ΦΠΑ. "]
["Περιλαμβάνει τις παρακάτω κατηγορίες υλικών:"]
["Βιομηχανικός αυτοματισμός Simatic και Υλικά Δικτύου (Simatic)\nΒιομηχανικός αυτοματισμός Simatic S71200 (S7-1200)\nLOGO!, τροφοδοτικά LOGO! Power (LOGO!)\nΚινητήρες Χαμηλής τάσης AC (LVM) \n",null,"Ηλεκτρολογικό Υλικό Χαμηλής Τάσης (LP) \nΡυθμιστές στροφών και συστήματα ελέγχου κίνησης  Motion control (MC)\nΒιομηχανικό υλικό χαμηλής τάσης (CP)"]
["Αναζήτηση υλικού","Αναζήτηση με:"]
["Κωδικός","Περιγραφή","Τιμή καταλόγου (€)","Μον. Μέτρησης","Ποσ. μονάδας μέτρησης","Κατηγορία υλικού","Ελάχιστη ποσότητα παραγγελίας"]
["1FK2102-0AG00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D8x25 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1048,"ΤΕΜ",1,"MC",1,"1FK21020AG000MA0"]
["1FK2102-0AG00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D8x25 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",739,"ΤΕΜ",1,"MC",1,"1FK21020AG000SA0"]
["1FK2102-0AG00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D8x25mm with fitted key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1048,"ΤΕΜ",1,"MC",1,"1FK21020AG001MA0"]
["1FK2102-0AG00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D8x25mm with fitted key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",739,"ΤΕΜ",1,"MC",1,"1FK21020AG001SA0"]
["1FK2102-0AG01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D8x25 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1134,"ΤΕΜ",1,"MC",1,"1FK21020AG010MA0"]
["1FK2102-0AG01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D8x25 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",825,"ΤΕΜ",1,"MC",1,"1FK21020AG010SA0"]
["1FK2102-0AG01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D8x25mm with fitted key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1134,"ΤΕΜ",1,"MC",1,"1FK21020AG011MA0"]
["1FK2102-0AG01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D8x25mm with fitted key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",825,"ΤΕΜ",1,"MC",1,"1FK21020AG011SA0"]
["1FK2102-0AG10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D8x25 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1254,"ΤΕΜ",1,"MC",1,"1FK21020AG100MA0"]
["1FK2102-0AG10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D8x25 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",945,"ΤΕΜ",1,"MC",1,"1FK21020AG100SA0"]
["1FK2102-0AG10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D8x25mm with fitted key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1254,"ΤΕΜ",1,"MC",1,"1FK21020AG101MA0"]
["1FK2102-0AG10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D8x25mm with fitted key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",945,"ΤΕΜ",1,"MC",1,"1FK21020AG101SA0"]
["1FK2102-0AG11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D8x25 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1340,"ΤΕΜ",1,"MC",1,"1FK21020AG110MA0"]
["1FK2102-0AG11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D8x25 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1031,"ΤΕΜ",1,"MC",1,"1FK21020AG110SA0"]
["1FK2102-0AG11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D8x25mm with fitted key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1340,"ΤΕΜ",1,"MC",1,"1FK21020AG111MA0"]
["1FK2102-0AG11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D8x25mm with fitted key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1031,"ΤΕΜ",1,"MC",1,"1FK21020AG111SA0"]
["1FK2102-1AG00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D8x25 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1068,"ΤΕΜ",1,"MC",1,"1FK21021AG000MA0"]
["1FK2102-1AG00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D8x25 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",760,"ΤΕΜ",1,"MC",1,"1FK21021AG000SA0"]
["1FK2102-1AG00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D8x25mm with fitted key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1068,"ΤΕΜ",1,"MC",1,"1FK21021AG001MA0"]
["1FK2102-1AG00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D8x25mm with fitted key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",760,"ΤΕΜ",1,"MC",1,"1FK21021AG001SA0"]
["1FK2102-1AG01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D8x25 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1154,"ΤΕΜ",1,"MC",1,"1FK21021AG010MA0"]
["1FK2102-1AG01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D8x25 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",846,"ΤΕΜ",1,"MC",1,"1FK21021AG010SA0"]
["1FK2102-1AG01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D8x25mm with fitted key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1154,"ΤΕΜ",1,"MC",1,"1FK21021AG011MA0"]
["1FK2102-1AG01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D8x25mm with fitted key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",846,"ΤΕΜ",1,"MC",1,"1FK21021AG011SA0"]
["1FK2102-1AG10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D8x25 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1274,"ΤΕΜ",1,"MC",1,"1FK21021AG100MA0"]
["1FK2102-1AG10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D8x25 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",966,"ΤΕΜ",1,"MC",1,"1FK21021AG100SA0"]
["1FK2102-1AG10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D8x25mm with fitted key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1274,"ΤΕΜ",1,"MC",1,"1FK21021AG101MA0"]
["1FK2102-1AG10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D8x25mm with fitted key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",966,"ΤΕΜ",1,"MC",1,"1FK21021AG101SA0"]
["1FK2102-1AG11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D8x25 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1361,"ΤΕΜ",1,"MC",1,"1FK21021AG110MA0"]
["1FK2102-1AG11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D8x25 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1052,"ΤΕΜ",1,"MC",1,"1FK21021AG110SA0"]
["1FK2102-1AG11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D8x25mm with fitted key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1361,"ΤΕΜ",1,"MC",1,"1FK21021AG111MA0"]
["1FK2102-1AG11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D8x25mm with fitted key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1052,"ΤΕΜ",1,"MC",1,"1FK21021AG111SA0"]
["1FK2103-2AG00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1130,"ΤΕΜ",1,"MC",1,"1FK21032AG000MA0"]
["1FK2103-2AG00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",821,"ΤΕΜ",1,"MC",1,"1FK21032AG000SA0"]
["1FK2103-2AG00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1130,"ΤΕΜ",1,"MC",1,"1FK21032AG001MA0"]
["1FK2103-2AG00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",821,"ΤΕΜ",1,"MC",1,"1FK21032AG001SA0"]
["1FK2103-2AG00-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1130,"ΤΕΜ",1,"MC",1,"1FK21032AG002MA0"]
["1FK2103-2AG00-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",821,"ΤΕΜ",1,"MC",1,"1FK21032AG002SA0"]
["1FK2103-2AG01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1216,"ΤΕΜ",1,"MC",1,"1FK21032AG010MA0"]
["1FK2103-2AG01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",907,"ΤΕΜ",1,"MC",1,"1FK21032AG010SA0"]
["1FK2103-2AG01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1216,"ΤΕΜ",1,"MC",1,"1FK21032AG011MA0"]
["1FK2103-2AG01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",907,"ΤΕΜ",1,"MC",1,"1FK21032AG011SA0"]
["1FK2103-2AG10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1377,"ΤΕΜ",1,"MC",1,"1FK21032AG100MA0"]
["1FK2103-2AG10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1069,"ΤΕΜ",1,"MC",1,"1FK21032AG100SA0"]
["1FK2103-2AG10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1377,"ΤΕΜ",1,"MC",1,"1FK21032AG101MA0"]
["1FK2103-2AG10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1069,"ΤΕΜ",1,"MC",1,"1FK21032AG101SA0"]
["1FK2103-2AG10-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1377,"ΤΕΜ",1,"MC",1,"1FK21032AG102MA0"]
["1FK2103-2AG10-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1069,"ΤΕΜ",1,"MC",1,"1FK21032AG102SA0"]
["1FK2103-2AG11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1463,"ΤΕΜ",1,"MC",1,"1FK21032AG110MA0"]
["1FK2103-2AG11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1155,"ΤΕΜ",1,"MC",1,"1FK21032AG110SA0"]
["1FK2103-2AG11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1463,"ΤΕΜ",1,"MC",1,"1FK21032AG111MA0"]
["1FK2103-2AG11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1155,"ΤΕΜ",1,"MC",1,"1FK21032AG111SA0"]
["1FK2103-4AG00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1253,"ΤΕΜ",1,"MC",1,"1FK21034AG000MA0"]
["1FK2103-4AG00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",944,"ΤΕΜ",1,"MC",1,"1FK21034AG000SA0"]
["1FK2103-4AG00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1253,"ΤΕΜ",1,"MC",1,"1FK21034AG001MA0"]
["1FK2103-4AG00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",944,"ΤΕΜ",1,"MC",1,"1FK21034AG001SA0"]
["1FK2103-4AG00-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1253,"ΤΕΜ",1,"MC",1,"1FK21034AG002MA0"]
["1FK2103-4AG00-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",944,"ΤΕΜ",1,"MC",1,"1FK21034AG002SA0"]
["1FK2103-4AG01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1339,"ΤΕΜ",1,"MC",1,"1FK21034AG010MA0"]
["1FK2103-4AG01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1030,"ΤΕΜ",1,"MC",1,"1FK21034AG010SA0"]
["1FK2103-4AG01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1339,"ΤΕΜ",1,"MC",1,"1FK21034AG011MA0"]
["1FK2103-4AG01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1030,"ΤΕΜ",1,"MC",1,"1FK21034AG011SA0"]
["1FK2103-4AG10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1500,"ΤΕΜ",1,"MC",1,"1FK21034AG100MA0"]
["1FK2103-4AG10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1192,"ΤΕΜ",1,"MC",1,"1FK21034AG100SA0"]
["1FK2103-4AG10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1500,"ΤΕΜ",1,"MC",1,"1FK21034AG101MA0"]
["1FK2103-4AG10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1192,"ΤΕΜ",1,"MC",1,"1FK21034AG101SA0"]
["1FK2103-4AG10-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1500,"ΤΕΜ",1,"MC",1,"1FK21034AG102MA0"]
["1FK2103-4AG10-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1192,"ΤΕΜ",1,"MC",1,"1FK21034AG102SA0"]
["1FK2103-4AG11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1587,"ΤΕΜ",1,"MC",1,"1FK21034AG110MA0"]
["1FK2103-4AG11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1278,"ΤΕΜ",1,"MC",1,"1FK21034AG110SA0"]
["1FK2103-4AG11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1587,"ΤΕΜ",1,"MC",1,"1FK21034AG111MA0"]
["1FK2103-4AG11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1278,"ΤΕΜ",1,"MC",1,"1FK21034AG111SA0"]
["1FK2104-4AF00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1253,"ΤΕΜ",1,"MC",1,"1FK21044AF000MA0"]
["1FK2104-4AF00-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1253,"ΤΕΜ",1,"MC",1,"1FK21044AF000MB0"]
["1FK2104-4AF00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",944,"ΤΕΜ",1,"MC",1,"1FK21044AF000SA0"]
["1FK2104-4AF00-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",944,"ΤΕΜ",1,"MC",1,"1FK21044AF000SB0"]
["1FK2104-4AF00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1253,"ΤΕΜ",1,"MC",1,"1FK21044AF001MA0"]
["1FK2104-4AF00-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1253,"ΤΕΜ",1,"MC",1,"1FK21044AF001MB0"]
["1FK2104-4AF00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",944,"ΤΕΜ",1,"MC",1,"1FK21044AF001SA0"]
["1FK2104-4AF00-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",944,"ΤΕΜ",1,"MC",1,"1FK21044AF001SB0"]
["1FK2104-4AF00-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1253,"ΤΕΜ",1,"MC",1,"1FK21044AF002MA0"]
["1FK2104-4AF00-2MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1253,"ΤΕΜ",1,"MC",1,"1FK21044AF002MB0"]
["1FK2104-4AF00-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",944,"ΤΕΜ",1,"MC",1,"1FK21044AF002SA0"]
["1FK2104-4AF00-2SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",944,"ΤΕΜ",1,"MC",1,"1FK21044AF002SB0"]
["1FK2104-4AF01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1339,"ΤΕΜ",1,"MC",1,"1FK21044AF010MA0"]
["1FK2104-4AF01-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1339,"ΤΕΜ",1,"MC",1,"1FK21044AF010MB0"]
["1FK2104-4AF01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1030,"ΤΕΜ",1,"MC",1,"1FK21044AF010SA0"]
["1FK2104-4AF01-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1030,"ΤΕΜ",1,"MC",1,"1FK21044AF010SB0"]
["1FK2104-4AF01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1339,"ΤΕΜ",1,"MC",1,"1FK21044AF011MA0"]
["1FK2104-4AF01-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1339,"ΤΕΜ",1,"MC",1,"1FK21044AF011MB0"]
["1FK2104-4AF01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1030,"ΤΕΜ",1,"MC",1,"1FK21044AF011SA0"]
["1FK2104-4AF01-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1030,"ΤΕΜ",1,"MC",1,"1FK21044AF011SB0"]
["1FK2104-4AF10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1500,"ΤΕΜ",1,"MC",1,"1FK21044AF100MA0"]
["1FK2104-4AF10-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1500,"ΤΕΜ",1,"MC",1,"1FK21044AF100MB0"]
["1FK2104-4AF10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1192,"ΤΕΜ",1,"MC",1,"1FK21044AF100SA0"]
["1FK2104-4AF10-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1192,"ΤΕΜ",1,"MC",1,"1FK21044AF100SB0"]
["1FK2104-4AF10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1500,"ΤΕΜ",1,"MC",1,"1FK21044AF101MA0"]
["1FK2104-4AF10-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1500,"ΤΕΜ",1,"MC",1,"1FK21044AF101MB0"]
["1FK2104-4AF10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1192,"ΤΕΜ",1,"MC",1,"1FK21044AF101SA0"]
["1FK2104-4AF10-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1192,"ΤΕΜ",1,"MC",1,"1FK21044AF101SB0"]
["1FK2104-4AF10-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1500,"ΤΕΜ",1,"MC",1,"1FK21044AF102MA0"]
["1FK2104-4AF10-2MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1500,"ΤΕΜ",1,"MC",1,"1FK21044AF102MB0"]
["1FK2104-4AF10-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1192,"ΤΕΜ",1,"MC",1,"1FK21044AF102SA0"]
["1FK2104-4AF10-2SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1192,"ΤΕΜ",1,"MC",1,"1FK21044AF102SB0"]
["1FK2104-4AF11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1587,"ΤΕΜ",1,"MC",1,"1FK21044AF110MA0"]
["1FK2104-4AF11-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1587,"ΤΕΜ",1,"MC",1,"1FK21044AF110MB0"]
["1FK2104-4AF11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1278,"ΤΕΜ",1,"MC",1,"1FK21044AF110SA0"]
["1FK2104-4AF11-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1278,"ΤΕΜ",1,"MC",1,"1FK21044AF110SB0"]
["1FK2104-4AF11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1587,"ΤΕΜ",1,"MC",1,"1FK21044AF111MA0"]
["1FK2104-4AF11-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1587,"ΤΕΜ",1,"MC",1,"1FK21044AF111MB0"]
["1FK2104-4AF11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1278,"ΤΕΜ",1,"MC",1,"1FK21044AF111SA0"]
["1FK2104-4AF11-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1278,"ΤΕΜ",1,"MC",1,"1FK21044AF111SB0"]
["1FK2104-4AK00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1253,"ΤΕΜ",1,"MC",1,"1FK21044AK000MA0"]
["1FK2104-4AK00-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1253,"ΤΕΜ",1,"MC",1,"1FK21044AK000MB0"]
["1FK2104-4AK00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",944,"ΤΕΜ",1,"MC",1,"1FK21044AK000SA0"]
["1FK2104-4AK00-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",944,"ΤΕΜ",1,"MC",1,"1FK21044AK000SB0"]
["1FK2104-4AK00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1253,"ΤΕΜ",1,"MC",1,"1FK21044AK001MA0"]
["1FK2104-4AK00-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1253,"ΤΕΜ",1,"MC",1,"1FK21044AK001MB0"]
["1FK2104-4AK00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",944,"ΤΕΜ",1,"MC",1,"1FK21044AK001SA0"]
["1FK2104-4AK00-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",944,"ΤΕΜ",1,"MC",1,"1FK21044AK001SB0"]
["1FK2104-4AK00-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1253,"ΤΕΜ",1,"MC",1,"1FK21044AK002MA0"]
["1FK2104-4AK00-2MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1253,"ΤΕΜ",1,"MC",1,"1FK21044AK002MB0"]
["1FK2104-4AK00-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",944,"ΤΕΜ",1,"MC",1,"1FK21044AK002SA0"]
["1FK2104-4AK00-2SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",944,"ΤΕΜ",1,"MC",1,"1FK21044AK002SB0"]
["1FK2104-4AK01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1339,"ΤΕΜ",1,"MC",1,"1FK21044AK010MA0"]
["1FK2104-4AK01-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1339,"ΤΕΜ",1,"MC",1,"1FK21044AK010MB0"]
["1FK2104-4AK01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1030,"ΤΕΜ",1,"MC",1,"1FK21044AK010SA0"]
["1FK2104-4AK01-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1030,"ΤΕΜ",1,"MC",1,"1FK21044AK010SB0"]
["1FK2104-4AK01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1339,"ΤΕΜ",1,"MC",1,"1FK21044AK011MA0"]
["1FK2104-4AK01-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1339,"ΤΕΜ",1,"MC",1,"1FK21044AK011MB0"]
["1FK2104-4AK01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1030,"ΤΕΜ",1,"MC",1,"1FK21044AK011SA0"]
["1FK2104-4AK01-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1030,"ΤΕΜ",1,"MC",1,"1FK21044AK011SB0"]
["1FK2104-4AK10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1500,"ΤΕΜ",1,"MC",1,"1FK21044AK100MA0"]
["1FK2104-4AK10-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1500,"ΤΕΜ",1,"MC",1,"1FK21044AK100MB0"]
["1FK2104-4AK10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1192,"ΤΕΜ",1,"MC",1,"1FK21044AK100SA0"]
["1FK2104-4AK10-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1192,"ΤΕΜ",1,"MC",1,"1FK21044AK100SB0"]
["1FK2104-4AK10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1500,"ΤΕΜ",1,"MC",1,"1FK21044AK101MA0"]
["1FK2104-4AK10-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1500,"ΤΕΜ",1,"MC",1,"1FK21044AK101MB0"]
["1FK2104-4AK10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1192,"ΤΕΜ",1,"MC",1,"1FK21044AK101SA0"]
["1FK2104-4AK10-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1192,"ΤΕΜ",1,"MC",1,"1FK21044AK101SB0"]
["1FK2104-4AK10-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1500,"ΤΕΜ",1,"MC",1,"1FK21044AK102MA0"]
["1FK2104-4AK10-2MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1500,"ΤΕΜ",1,"MC",1,"1FK21044AK102MB0"]
["1FK2104-4AK10-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1192,"ΤΕΜ",1,"MC",1,"1FK21044AK102SA0"]
["1FK2104-4AK10-2SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1192,"ΤΕΜ",1,"MC",1,"1FK21044AK102SB0"]
["1FK2104-4AK11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1587,"ΤΕΜ",1,"MC",1,"1FK21044AK110MA0"]
["1FK2104-4AK11-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1587,"ΤΕΜ",1,"MC",1,"1FK21044AK110MB0"]
["1FK2104-4AK11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1278,"ΤΕΜ",1,"MC",1,"1FK21044AK110SA0"]
["1FK2104-4AK11-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1278,"ΤΕΜ",1,"MC",1,"1FK21044AK110SB0"]
["1FK2104-4AK11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1587,"ΤΕΜ",1,"MC",1,"1FK21044AK111MA0"]
["1FK2104-4AK11-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1587,"ΤΕΜ",1,"MC",1,"1FK21044AK111MB0"]
["1FK2104-4AK11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1278,"ΤΕΜ",1,"MC",1,"1FK21044AK111SA0"]
["1FK2104-4AK11-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1278,"ΤΕΜ",1,"MC",1,"1FK21044AK111SB0"]
["1FK2104-5AF00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1355,"ΤΕΜ",1,"MC",1,"1FK21045AF000MA0"]
["1FK2104-5AF00-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1355,"ΤΕΜ",1,"MC",1,"1FK21045AF000MB0"]
["1FK2104-5AF00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1047,"ΤΕΜ",1,"MC",1,"1FK21045AF000SA0"]
["1FK2104-5AF00-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1047,"ΤΕΜ",1,"MC",1,"1FK21045AF000SB0"]
["1FK2104-5AF00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1355,"ΤΕΜ",1,"MC",1,"1FK21045AF001MA0"]
["1FK2104-5AF00-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1355,"ΤΕΜ",1,"MC",1,"1FK21045AF001MB0"]
["1FK2104-5AF00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1047,"ΤΕΜ",1,"MC",1,"1FK21045AF001SA0"]
["1FK2104-5AF00-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1047,"ΤΕΜ",1,"MC",1,"1FK21045AF001SB0"]
["1FK2104-5AF00-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1355,"ΤΕΜ",1,"MC",1,"1FK21045AF002MA0"]
["1FK2104-5AF00-2MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1355,"ΤΕΜ",1,"MC",1,"1FK21045AF002MB0"]
["1FK2104-5AF00-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1047,"ΤΕΜ",1,"MC",1,"1FK21045AF002SA0"]
["1FK2104-5AF00-2SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1047,"ΤΕΜ",1,"MC",1,"1FK21045AF002SB0"]
["1FK2104-5AF01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1442,"ΤΕΜ",1,"MC",1,"1FK21045AF010MA0"]
["1FK2104-5AF01-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1442,"ΤΕΜ",1,"MC",1,"1FK21045AF010MB0"]
["1FK2104-5AF01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1133,"ΤΕΜ",1,"MC",1,"1FK21045AF010SA0"]
["1FK2104-5AF01-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1133,"ΤΕΜ",1,"MC",1,"1FK21045AF010SB0"]
["1FK2104-5AF01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1442,"ΤΕΜ",1,"MC",1,"1FK21045AF011MA0"]
["1FK2104-5AF01-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1442,"ΤΕΜ",1,"MC",1,"1FK21045AF011MB0"]
["1FK2104-5AF01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1133,"ΤΕΜ",1,"MC",1,"1FK21045AF011SA0"]
["1FK2104-5AF01-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1133,"ΤΕΜ",1,"MC",1,"1FK21045AF011SB0"]
["1FK2104-5AF10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1603,"ΤΕΜ",1,"MC",1,"1FK21045AF100MA0"]
["1FK2104-5AF10-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1603,"ΤΕΜ",1,"MC",1,"1FK21045AF100MB0"]
["1FK2104-5AF10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1294,"ΤΕΜ",1,"MC",1,"1FK21045AF100SA0"]
["1FK2104-5AF10-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1294,"ΤΕΜ",1,"MC",1,"1FK21045AF100SB0"]
["1FK2104-5AF10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1603,"ΤΕΜ",1,"MC",1,"1FK21045AF101MA0"]
["1FK2104-5AF10-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1603,"ΤΕΜ",1,"MC",1,"1FK21045AF101MB0"]
["1FK2104-5AF10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1294,"ΤΕΜ",1,"MC",1,"1FK21045AF101SA0"]
["1FK2104-5AF10-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1294,"ΤΕΜ",1,"MC",1,"1FK21045AF101SB0"]
["1FK2104-5AF10-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1603,"ΤΕΜ",1,"MC",1,"1FK21045AF102MA0"]
["1FK2104-5AF10-2MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1603,"ΤΕΜ",1,"MC",1,"1FK21045AF102MB0"]
["1FK2104-5AF10-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1294,"ΤΕΜ",1,"MC",1,"1FK21045AF102SA0"]
["1FK2104-5AF10-2SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1294,"ΤΕΜ",1,"MC",1,"1FK21045AF102SB0"]
["1FK2104-5AF11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1689,"ΤΕΜ",1,"MC",1,"1FK21045AF110MA0"]
["1FK2104-5AF11-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1689,"ΤΕΜ",1,"MC",1,"1FK21045AF110MB0"]
["1FK2104-5AF11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1380,"ΤΕΜ",1,"MC",1,"1FK21045AF110SA0"]
["1FK2104-5AF11-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1380,"ΤΕΜ",1,"MC",1,"1FK21045AF110SB0"]
["1FK2104-5AF11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1689,"ΤΕΜ",1,"MC",1,"1FK21045AF111MA0"]
["1FK2104-5AF11-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1689,"ΤΕΜ",1,"MC",1,"1FK21045AF111MB0"]
["1FK2104-5AF11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1380,"ΤΕΜ",1,"MC",1,"1FK21045AF111SA0"]
["1FK2104-5AF11-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1380,"ΤΕΜ",1,"MC",1,"1FK21045AF111SB0"]
["1FK2104-5AK00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1355,"ΤΕΜ",1,"MC",1,"1FK21045AK000MA0"]
["1FK2104-5AK00-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1355,"ΤΕΜ",1,"MC",1,"1FK21045AK000MB0"]
["1FK2104-5AK00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1047,"ΤΕΜ",1,"MC",1,"1FK21045AK000SA0"]
["1FK2104-5AK00-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1047,"ΤΕΜ",1,"MC",1,"1FK21045AK000SB0"]
["1FK2104-5AK00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1355,"ΤΕΜ",1,"MC",1,"1FK21045AK001MA0"]
["1FK2104-5AK00-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1355,"ΤΕΜ",1,"MC",1,"1FK21045AK001MB0"]
["1FK2104-5AK00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1047,"ΤΕΜ",1,"MC",1,"1FK21045AK001SA0"]
["1FK2104-5AK00-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1047,"ΤΕΜ",1,"MC",1,"1FK21045AK001SB0"]
["1FK2104-5AK00-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1355,"ΤΕΜ",1,"MC",1,"1FK21045AK002MA0"]
["1FK2104-5AK00-2MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1355,"ΤΕΜ",1,"MC",1,"1FK21045AK002MB0"]
["1FK2104-5AK00-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1047,"ΤΕΜ",1,"MC",1,"1FK21045AK002SA0"]
["1FK2104-5AK00-2SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1047,"ΤΕΜ",1,"MC",1,"1FK21045AK002SB0"]
["1FK2104-5AK01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1442,"ΤΕΜ",1,"MC",1,"1FK21045AK010MA0"]
["1FK2104-5AK01-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1442,"ΤΕΜ",1,"MC",1,"1FK21045AK010MB0"]
["1FK2104-5AK01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1133,"ΤΕΜ",1,"MC",1,"1FK21045AK010SA0"]
["1FK2104-5AK01-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1133,"ΤΕΜ",1,"MC",1,"1FK21045AK010SB0"]
["1FK2104-5AK01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1442,"ΤΕΜ",1,"MC",1,"1FK21045AK011MA0"]
["1FK2104-5AK01-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1442,"ΤΕΜ",1,"MC",1,"1FK21045AK011MB0"]
["1FK2104-5AK01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1133,"ΤΕΜ",1,"MC",1,"1FK21045AK011SA0"]
["1FK2104-5AK01-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1133,"ΤΕΜ",1,"MC",1,"1FK21045AK011SB0"]
["1FK2104-5AK10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1603,"ΤΕΜ",1,"MC",1,"1FK21045AK100MA0"]
["1FK2104-5AK10-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1603,"ΤΕΜ",1,"MC",1,"1FK21045AK100MB0"]
["1FK2104-5AK10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1294,"ΤΕΜ",1,"MC",1,"1FK21045AK100SA0"]
["1FK2104-5AK10-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1294,"ΤΕΜ",1,"MC",1,"1FK21045AK100SB0"]
["1FK2104-5AK10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1603,"ΤΕΜ",1,"MC",1,"1FK21045AK101MA0"]
["1FK2104-5AK10-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1603,"ΤΕΜ",1,"MC",1,"1FK21045AK101MB0"]
["1FK2104-5AK10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1294,"ΤΕΜ",1,"MC",1,"1FK21045AK101SA0"]
["1FK2104-5AK10-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1294,"ΤΕΜ",1,"MC",1,"1FK21045AK101SB0"]
["1FK2104-5AK10-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1603,"ΤΕΜ",1,"MC",1,"1FK21045AK102MA0"]
["1FK2104-5AK10-2MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1603,"ΤΕΜ",1,"MC",1,"1FK21045AK102MB0"]
["1FK2104-5AK10-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1294,"ΤΕΜ",1,"MC",1,"1FK21045AK102SA0"]
["1FK2104-5AK10-2SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1294,"ΤΕΜ",1,"MC",1,"1FK21045AK102SB0"]
["1FK2104-5AK11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1689,"ΤΕΜ",1,"MC",1,"1FK21045AK110MA0"]
["1FK2104-5AK11-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1689,"ΤΕΜ",1,"MC",1,"1FK21045AK110MB0"]
["1FK2104-5AK11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1380,"ΤΕΜ",1,"MC",1,"1FK21045AK110SA0"]
["1FK2104-5AK11-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1380,"ΤΕΜ",1,"MC",1,"1FK21045AK110SB0"]
["1FK2104-5AK11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1689,"ΤΕΜ",1,"MC",1,"1FK21045AK111MA0"]
["1FK2104-5AK11-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1689,"ΤΕΜ",1,"MC",1,"1FK21045AK111MB0"]
["1FK2104-5AK11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1380,"ΤΕΜ",1,"MC",1,"1FK21045AK111SA0"]
["1FK2104-5AK11-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1380,"ΤΕΜ",1,"MC",1,"1FK21045AK111SB0"]
["1FK2104-6AF00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1417,"ΤΕΜ",1,"MC",1,"1FK21046AF000MA0"]
["1FK2104-6AF00-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1417,"ΤΕΜ",1,"MC",1,"1FK21046AF000MB0"]
["1FK2104-6AF00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1108,"ΤΕΜ",1,"MC",1,"1FK21046AF000SA0"]
["1FK2104-6AF00-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1108,"ΤΕΜ",1,"MC",1,"1FK21046AF000SB0"]
["1FK2104-6AF00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1417,"ΤΕΜ",1,"MC",1,"1FK21046AF001MA0"]
["1FK2104-6AF00-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1417,"ΤΕΜ",1,"MC",1,"1FK21046AF001MB0"]
["1FK2104-6AF00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1108,"ΤΕΜ",1,"MC",1,"1FK21046AF001SA0"]
["1FK2104-6AF00-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1108,"ΤΕΜ",1,"MC",1,"1FK21046AF001SB0"]
["1FK2104-6AF00-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1417,"ΤΕΜ",1,"MC",1,"1FK21046AF002MA0"]
["1FK2104-6AF00-2MB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1417,"ΤΕΜ",1,"MC",1,"1FK21046AF002MB0"]
["1FK2104-6AF00-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1108,"ΤΕΜ",1,"MC",1,"1FK21046AF002SA0"]
["1FK2104-6AF00-2SB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1108,"ΤΕΜ",1,"MC",1,"1FK21046AF002SB0"]
["1FK2104-6AF01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1503,"ΤΕΜ",1,"MC",1,"1FK21046AF010MA0"]
["1FK2104-6AF01-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1503,"ΤΕΜ",1,"MC",1,"1FK21046AF010MB0"]
["1FK2104-6AF01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1195,"ΤΕΜ",1,"MC",1,"1FK21046AF010SA0"]
["1FK2104-6AF01-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1195,"ΤΕΜ",1,"MC",1,"1FK21046AF010SB0"]
["1FK2104-6AF01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1503,"ΤΕΜ",1,"MC",1,"1FK21046AF011MA0"]
["1FK2104-6AF01-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1503,"ΤΕΜ",1,"MC",1,"1FK21046AF011MB0"]
["1FK2104-6AF01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1195,"ΤΕΜ",1,"MC",1,"1FK21046AF011SA0"]
["1FK2104-6AF01-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1195,"ΤΕΜ",1,"MC",1,"1FK21046AF011SB0"]
["1FK2104-6AF10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1664,"ΤΕΜ",1,"MC",1,"1FK21046AF100MA0"]
["1FK2104-6AF10-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1664,"ΤΕΜ",1,"MC",1,"1FK21046AF100MB0"]
["1FK2104-6AF10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1356,"ΤΕΜ",1,"MC",1,"1FK21046AF100SA0"]
["1FK2104-6AF10-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1356,"ΤΕΜ",1,"MC",1,"1FK21046AF100SB0"]
["1FK2104-6AF10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1664,"ΤΕΜ",1,"MC",1,"1FK21046AF101MA0"]
["1FK2104-6AF10-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1664,"ΤΕΜ",1,"MC",1,"1FK21046AF101MB0"]
["1FK2104-6AF10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1356,"ΤΕΜ",1,"MC",1,"1FK21046AF101SA0"]
["1FK2104-6AF10-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1356,"ΤΕΜ",1,"MC",1,"1FK21046AF101SB0"]
["1FK2104-6AF10-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1664,"ΤΕΜ",1,"MC",1,"1FK21046AF102MA0"]
["1FK2104-6AF10-2MB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1664,"ΤΕΜ",1,"MC",1,"1FK21046AF102MB0"]
["1FK2104-6AF10-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1356,"ΤΕΜ",1,"MC",1,"1FK21046AF102SA0"]
["1FK2104-6AF10-2SB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1356,"ΤΕΜ",1,"MC",1,"1FK21046AF102SB0"]
["1FK2104-6AF11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1751,"ΤΕΜ",1,"MC",1,"1FK21046AF110MA0"]
["1FK2104-6AF11-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1751,"ΤΕΜ",1,"MC",1,"1FK21046AF110MB0"]
["1FK2104-6AF11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1442,"ΤΕΜ",1,"MC",1,"1FK21046AF110SA0"]
["1FK2104-6AF11-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1442,"ΤΕΜ",1,"MC",1,"1FK21046AF110SB0"]
["1FK2104-6AF11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1751,"ΤΕΜ",1,"MC",1,"1FK21046AF111MA0"]
["1FK2104-6AF11-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1751,"ΤΕΜ",1,"MC",1,"1FK21046AF111MB0"]
["1FK2104-6AF11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1442,"ΤΕΜ",1,"MC",1,"1FK21046AF111SA0"]
["1FK2104-6AF11-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1442,"ΤΕΜ",1,"MC",1,"1FK21046AF111SB0"]
["1FK2105-4AF00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1577,"ΤΕΜ",1,"MC",1,"1FK21054AF000MA0"]
["1FK2105-4AF00-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1577,"ΤΕΜ",1,"MC",1,"1FK21054AF000MB0"]
["1FK2105-4AF00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1269,"ΤΕΜ",1,"MC",1,"1FK21054AF000SA0"]
["1FK2105-4AF00-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1269,"ΤΕΜ",1,"MC",1,"1FK21054AF000SB0"]
["1FK2105-4AF00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1577,"ΤΕΜ",1,"MC",1,"1FK21054AF001MA0"]
["1FK2105-4AF00-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1577,"ΤΕΜ",1,"MC",1,"1FK21054AF001MB0"]
["1FK2105-4AF00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1269,"ΤΕΜ",1,"MC",1,"1FK21054AF001SA0"]
["1FK2105-4AF00-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1269,"ΤΕΜ",1,"MC",1,"1FK21054AF001SB0"]
["1FK2105-4AF01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1663,"ΤΕΜ",1,"MC",1,"1FK21054AF010MA0"]
["1FK2105-4AF01-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1663,"ΤΕΜ",1,"MC",1,"1FK21054AF010MB0"]
["1FK2105-4AF01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1355,"ΤΕΜ",1,"MC",1,"1FK21054AF010SA0"]
["1FK2105-4AF01-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1355,"ΤΕΜ",1,"MC",1,"1FK21054AF010SB0"]
["1FK2105-4AF01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1663,"ΤΕΜ",1,"MC",1,"1FK21054AF011MA0"]
["1FK2105-4AF01-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1663,"ΤΕΜ",1,"MC",1,"1FK21054AF011MB0"]
["1FK2105-4AF01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1355,"ΤΕΜ",1,"MC",1,"1FK21054AF011SA0"]
["1FK2105-4AF01-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1355,"ΤΕΜ",1,"MC",1,"1FK21054AF011SB0"]
["1FK2105-4AF10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1866,"ΤΕΜ",1,"MC",1,"1FK21054AF100MA0"]
["1FK2105-4AF10-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1866,"ΤΕΜ",1,"MC",1,"1FK21054AF100MB0"]
["1FK2105-4AF10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1557,"ΤΕΜ",1,"MC",1,"1FK21054AF100SA0"]
["1FK2105-4AF10-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1557,"ΤΕΜ",1,"MC",1,"1FK21054AF100SB0"]
["1FK2105-4AF10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1866,"ΤΕΜ",1,"MC",1,"1FK21054AF101MA0"]
["1FK2105-4AF10-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1866,"ΤΕΜ",1,"MC",1,"1FK21054AF101MB0"]
["1FK2105-4AF10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1557,"ΤΕΜ",1,"MC",1,"1FK21054AF101SA0"]
["1FK2105-4AF10-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1557,"ΤΕΜ",1,"MC",1,"1FK21054AF101SB0"]
["1FK2105-4AF11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1952,"ΤΕΜ",1,"MC",1,"1FK21054AF110MA0"]
["1FK2105-4AF11-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1952,"ΤΕΜ",1,"MC",1,"1FK21054AF110MB0"]
["1FK2105-4AF11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1643,"ΤΕΜ",1,"MC",1,"1FK21054AF110SA0"]
["1FK2105-4AF11-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1643,"ΤΕΜ",1,"MC",1,"1FK21054AF110SB0"]
["1FK2105-4AF11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1952,"ΤΕΜ",1,"MC",1,"1FK21054AF111MA0"]
["1FK2105-4AF11-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1952,"ΤΕΜ",1,"MC",1,"1FK21054AF111MB0"]
["1FK2105-4AF11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1643,"ΤΕΜ",1,"MC",1,"1FK21054AF111SA0"]
["1FK2105-4AF11-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1643,"ΤΕΜ",1,"MC",1,"1FK21054AF111SB0"]
["1FK2105-6AF00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1827,"ΤΕΜ",1,"MC",1,"1FK21056AF000MA0"]
["1FK2105-6AF00-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1827,"ΤΕΜ",1,"MC",1,"1FK21056AF000MB0"]
["1FK2105-6AF00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1519,"ΤΕΜ",1,"MC",1,"1FK21056AF000SA0"]
["1FK2105-6AF00-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1519,"ΤΕΜ",1,"MC",1,"1FK21056AF000SB0"]
["1FK2105-6AF00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1827,"ΤΕΜ",1,"MC",1,"1FK21056AF001MA0"]
["1FK2105-6AF00-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1827,"ΤΕΜ",1,"MC",1,"1FK21056AF001MB0"]
["1FK2105-6AF00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1519,"ΤΕΜ",1,"MC",1,"1FK21056AF001SA0"]
["1FK2105-6AF00-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1519,"ΤΕΜ",1,"MC",1,"1FK21056AF001SB0"]
["1FK2105-6AF01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1914,"ΤΕΜ",1,"MC",1,"1FK21056AF010MA0"]
["1FK2105-6AF01-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1914,"ΤΕΜ",1,"MC",1,"1FK21056AF010MB0"]
["1FK2105-6AF01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1605,"ΤΕΜ",1,"MC",1,"1FK21056AF010SA0"]
["1FK2105-6AF01-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1605,"ΤΕΜ",1,"MC",1,"1FK21056AF010SB0"]
["1FK2105-6AF01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1914,"ΤΕΜ",1,"MC",1,"1FK21056AF011MA0"]
["1FK2105-6AF01-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1914,"ΤΕΜ",1,"MC",1,"1FK21056AF011MB0"]
["1FK2105-6AF01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1605,"ΤΕΜ",1,"MC",1,"1FK21056AF011SA0"]
["1FK2105-6AF01-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1605,"ΤΕΜ",1,"MC",1,"1FK21056AF011SB0"]
["1FK2105-6AF10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",2116,"ΤΕΜ",1,"MC",1,"1FK21056AF100MA0"]
["1FK2105-6AF10-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",2116,"ΤΕΜ",1,"MC",1,"1FK21056AF100MB0"]
["1FK2105-6AF10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1807,"ΤΕΜ",1,"MC",1,"1FK21056AF100SA0"]
["1FK2105-6AF10-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1807,"ΤΕΜ",1,"MC",1,"1FK21056AF100SB0"]
["1FK2105-6AF10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",2116,"ΤΕΜ",1,"MC",1,"1FK21056AF101MA0"]
["1FK2105-6AF10-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",2116,"ΤΕΜ",1,"MC",1,"1FK21056AF101MB0"]
["1FK2105-6AF10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1807,"ΤΕΜ",1,"MC",1,"1FK21056AF101SA0"]
["1FK2105-6AF10-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1807,"ΤΕΜ",1,"MC",1,"1FK21056AF101SB0"]
["1FK2105-6AF11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",2202,"ΤΕΜ",1,"MC",1,"1FK21056AF110MA0"]
["1FK2105-6AF11-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",2202,"ΤΕΜ",1,"MC",1,"1FK21056AF110MB0"]
["1FK2105-6AF11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1894,"ΤΕΜ",1,"MC",1,"1FK21056AF110SA0"]
["1FK2105-6AF11-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1894,"ΤΕΜ",1,"MC",1,"1FK21056AF110SB0"]
["1FK2105-6AF11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",2202,"ΤΕΜ",1,"MC",1,"1FK21056AF111MA0"]
["1FK2105-6AF11-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",2202,"ΤΕΜ",1,"MC",1,"1FK21056AF111MB0"]
["1FK2105-6AF11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1894,"ΤΕΜ",1,"MC",1,"1FK21056AF111SA0"]
["1FK2105-6AF11-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1894,"ΤΕΜ",1,"MC",1,"1FK21056AF111SB0"]
["1FK2106-3AF00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",1885,"ΤΕΜ",1,"MC",1,"1FK21063AF000MA0"]
["1FK2106-3AF00-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1885,"ΤΕΜ",1,"MC",1,"1FK21063AF000MB0"]
["1FK2106-3AF00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1576,"ΤΕΜ",1,"MC",1,"1FK21063AF000SA0"]
["1FK2106-3AF00-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1576,"ΤΕΜ",1,"MC",1,"1FK21063AF000SB0"]
["1FK2106-3AF00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",1885,"ΤΕΜ",1,"MC",1,"1FK21063AF001MA0"]
["1FK2106-3AF00-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1885,"ΤΕΜ",1,"MC",1,"1FK21063AF001MB0"]
["1FK2106-3AF00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1576,"ΤΕΜ",1,"MC",1,"1FK21063AF001SA0"]
["1FK2106-3AF00-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1576,"ΤΕΜ",1,"MC",1,"1FK21063AF001SB0"]
["1FK2106-3AF01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",1971,"ΤΕΜ",1,"MC",1,"1FK21063AF010MA0"]
["1FK2106-3AF01-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1971,"ΤΕΜ",1,"MC",1,"1FK21063AF010MB0"]
["1FK2106-3AF01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1662,"ΤΕΜ",1,"MC",1,"1FK21063AF010SA0"]
["1FK2106-3AF01-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1662,"ΤΕΜ",1,"MC",1,"1FK21063AF010SB0"]
["1FK2106-3AF01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",1971,"ΤΕΜ",1,"MC",1,"1FK21063AF011MA0"]
["1FK2106-3AF01-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1971,"ΤΕΜ",1,"MC",1,"1FK21063AF011MB0"]
["1FK2106-3AF01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1662,"ΤΕΜ",1,"MC",1,"1FK21063AF011SA0"]
["1FK2106-3AF01-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1662,"ΤΕΜ",1,"MC",1,"1FK21063AF011SB0"]
["1FK2106-3AF10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2215,"ΤΕΜ",1,"MC",1,"1FK21063AF100MA0"]
["1FK2106-3AF10-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2215,"ΤΕΜ",1,"MC",1,"1FK21063AF100MB0"]
["1FK2106-3AF10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1906,"ΤΕΜ",1,"MC",1,"1FK21063AF100SA0"]
["1FK2106-3AF10-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1906,"ΤΕΜ",1,"MC",1,"1FK21063AF100SB0"]
["1FK2106-3AF10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2215,"ΤΕΜ",1,"MC",1,"1FK21063AF101MA0"]
["1FK2106-3AF10-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2215,"ΤΕΜ",1,"MC",1,"1FK21063AF101MB0"]
["1FK2106-3AF10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1906,"ΤΕΜ",1,"MC",1,"1FK21063AF101SA0"]
["1FK2106-3AF10-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1906,"ΤΕΜ",1,"MC",1,"1FK21063AF101SB0"]
["1FK2106-3AF11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2301,"ΤΕΜ",1,"MC",1,"1FK21063AF110MA0"]
["1FK2106-3AF11-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2301,"ΤΕΜ",1,"MC",1,"1FK21063AF110MB0"]
["1FK2106-3AF11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1992,"ΤΕΜ",1,"MC",1,"1FK21063AF110SA0"]
["1FK2106-3AF11-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1992,"ΤΕΜ",1,"MC",1,"1FK21063AF110SB0"]
["1FK2106-3AF11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2301,"ΤΕΜ",1,"MC",1,"1FK21063AF111MA0"]
["1FK2106-3AF11-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2301,"ΤΕΜ",1,"MC",1,"1FK21063AF111MB0"]
["1FK2106-3AF11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1992,"ΤΕΜ",1,"MC",1,"1FK21063AF111SA0"]
["1FK2106-3AF11-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1992,"ΤΕΜ",1,"MC",1,"1FK21063AF111SB0"]
["1FK2106-4AF00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2027,"ΤΕΜ",1,"MC",1,"1FK21064AF000MA0"]
["1FK2106-4AF00-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2027,"ΤΕΜ",1,"MC",1,"1FK21064AF000MB0"]
["1FK2106-4AF00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1718,"ΤΕΜ",1,"MC",1,"1FK21064AF000SA0"]
["1FK2106-4AF00-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1718,"ΤΕΜ",1,"MC",1,"1FK21064AF000SB0"]
["1FK2106-4AF00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2027,"ΤΕΜ",1,"MC",1,"1FK21064AF001MA0"]
["1FK2106-4AF00-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2027,"ΤΕΜ",1,"MC",1,"1FK21064AF001MB0"]
["1FK2106-4AF00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1718,"ΤΕΜ",1,"MC",1,"1FK21064AF001SA0"]
["1FK2106-4AF00-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1718,"ΤΕΜ",1,"MC",1,"1FK21064AF001SB0"]
["1FK2106-4AF01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2113,"ΤΕΜ",1,"MC",1,"1FK21064AF010MA0"]
["1FK2106-4AF01-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2113,"ΤΕΜ",1,"MC",1,"1FK21064AF010MB0"]
["1FK2106-4AF01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1804,"ΤΕΜ",1,"MC",1,"1FK21064AF010SA0"]
["1FK2106-4AF01-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1804,"ΤΕΜ",1,"MC",1,"1FK21064AF010SB0"]
["1FK2106-4AF01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2113,"ΤΕΜ",1,"MC",1,"1FK21064AF011MA0"]
["1FK2106-4AF01-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2113,"ΤΕΜ",1,"MC",1,"1FK21064AF011MB0"]
["1FK2106-4AF01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1804,"ΤΕΜ",1,"MC",1,"1FK21064AF011SA0"]
["1FK2106-4AF01-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1804,"ΤΕΜ",1,"MC",1,"1FK21064AF011SB0"]
["1FK2106-4AF10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2357,"ΤΕΜ",1,"MC",1,"1FK21064AF100MA0"]
["1FK2106-4AF10-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2357,"ΤΕΜ",1,"MC",1,"1FK21064AF100MB0"]
["1FK2106-4AF10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2048,"ΤΕΜ",1,"MC",1,"1FK21064AF100SA0"]
["1FK2106-4AF10-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2048,"ΤΕΜ",1,"MC",1,"1FK21064AF100SB0"]
["1FK2106-4AF10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2357,"ΤΕΜ",1,"MC",1,"1FK21064AF101MA0"]
["1FK2106-4AF10-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2357,"ΤΕΜ",1,"MC",1,"1FK21064AF101MB0"]
["1FK2106-4AF10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2048,"ΤΕΜ",1,"MC",1,"1FK21064AF101SA0"]
["1FK2106-4AF10-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2048,"ΤΕΜ",1,"MC",1,"1FK21064AF101SB0"]
["1FK2106-4AF11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2443,"ΤΕΜ",1,"MC",1,"1FK21064AF110MA0"]
["1FK2106-4AF11-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2443,"ΤΕΜ",1,"MC",1,"1FK21064AF110MB0"]
["1FK2106-4AF11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2134,"ΤΕΜ",1,"MC",1,"1FK21064AF110SA0"]
["1FK2106-4AF11-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2134,"ΤΕΜ",1,"MC",1,"1FK21064AF110SB0"]
["1FK2106-4AF11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2443,"ΤΕΜ",1,"MC",1,"1FK21064AF111MA0"]
["1FK2106-4AF11-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2443,"ΤΕΜ",1,"MC",1,"1FK21064AF111MB0"]
["1FK2106-4AF11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2134,"ΤΕΜ",1,"MC",1,"1FK21064AF111SA0"]
["1FK2106-4AF11-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2134,"ΤΕΜ",1,"MC",1,"1FK21064AF111SB0"]
["1FK2106-6AF00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2331,"ΤΕΜ",1,"MC",1,"1FK21066AF000MA0"]
["1FK2106-6AF00-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2331,"ΤΕΜ",1,"MC",1,"1FK21066AF000MB0"]
["1FK2106-6AF00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2022,"ΤΕΜ",1,"MC",1,"1FK21066AF000SA0"]
["1FK2106-6AF00-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2022,"ΤΕΜ",1,"MC",1,"1FK21066AF000SB0"]
["1FK2106-6AF00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2331,"ΤΕΜ",1,"MC",1,"1FK21066AF001MA0"]
["1FK2106-6AF00-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2331,"ΤΕΜ",1,"MC",1,"1FK21066AF001MB0"]
["1FK2106-6AF00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2022,"ΤΕΜ",1,"MC",1,"1FK21066AF001SA0"]
["1FK2106-6AF00-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2022,"ΤΕΜ",1,"MC",1,"1FK21066AF001SB0"]
["1FK2106-6AF01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2417,"ΤΕΜ",1,"MC",1,"1FK21066AF010MA0"]
["1FK2106-6AF01-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2417,"ΤΕΜ",1,"MC",1,"1FK21066AF010MB0"]
["1FK2106-6AF01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2108,"ΤΕΜ",1,"MC",1,"1FK21066AF010SA0"]
["1FK2106-6AF01-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2108,"ΤΕΜ",1,"MC",1,"1FK21066AF010SB0"]
["1FK2106-6AF01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2417,"ΤΕΜ",1,"MC",1,"1FK21066AF011MA0"]
["1FK2106-6AF01-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2417,"ΤΕΜ",1,"MC",1,"1FK21066AF011MB0"]
["1FK2106-6AF01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2108,"ΤΕΜ",1,"MC",1,"1FK21066AF011SA0"]
["1FK2106-6AF01-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2108,"ΤΕΜ",1,"MC",1,"1FK21066AF011SB0"]
["1FK2106-6AF10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2661,"ΤΕΜ",1,"MC",1,"1FK21066AF100MA0"]
["1FK2106-6AF10-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2661,"ΤΕΜ",1,"MC",1,"1FK21066AF100MB0"]
["1FK2106-6AF10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2352,"ΤΕΜ",1,"MC",1,"1FK21066AF100SA0"]
["1FK2106-6AF10-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2352,"ΤΕΜ",1,"MC",1,"1FK21066AF100SB0"]
["1FK2106-6AF10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2661,"ΤΕΜ",1,"MC",1,"1FK21066AF101MA0"]
["1FK2106-6AF10-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2661,"ΤΕΜ",1,"MC",1,"1FK21066AF101MB0"]
["1FK2106-6AF10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2352,"ΤΕΜ",1,"MC",1,"1FK21066AF101SA0"]
["1FK2106-6AF10-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2352,"ΤΕΜ",1,"MC",1,"1FK21066AF101SB0"]
["1FK2106-6AF11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2747,"ΤΕΜ",1,"MC",1,"1FK21066AF110MA0"]
["1FK2106-6AF11-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2747,"ΤΕΜ",1,"MC",1,"1FK21066AF110MB0"]
["1FK2106-6AF11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2438,"ΤΕΜ",1,"MC",1,"1FK21066AF110SA0"]
["1FK2106-6AF11-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2438,"ΤΕΜ",1,"MC",1,"1FK21066AF110SB0"]
["1FK2106-6AF11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2747,"ΤΕΜ",1,"MC",1,"1FK21066AF111MA0"]
["1FK2106-6AF11-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2747,"ΤΕΜ",1,"MC",1,"1FK21066AF111MB0"]
["1FK2106-6AF11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2438,"ΤΕΜ",1,"MC",1,"1FK21066AF111SA0"]
["1FK2106-6AF11-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2438,"ΤΕΜ",1,"MC",1,"1FK21066AF111SB0"]
["1FK2203-2AG00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1130,"ΤΕΜ",1,"MC",1,"1FK22032AG000MA0"]
["1FK2203-2AG00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",821,"ΤΕΜ",1,"MC",1,"1FK22032AG000SA0"]
["1FK2203-2AG00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1130,"ΤΕΜ",1,"MC",1,"1FK22032AG001MA0"]
["1FK2203-2AG00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",821,"ΤΕΜ",1,"MC",1,"1FK22032AG001SA0"]
["1FK2203-2AG00-2MA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1130,"ΤΕΜ",1,"MC",1,"1FK22032AG002MA0"]
["1FK2203-2AG00-2SA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",821,"ΤΕΜ",1,"MC",1,"1FK22032AG002SA0"]
["1FK2203-2AG01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1216,"ΤΕΜ",1,"MC",1,"1FK22032AG010MA0"]
["1FK2203-2AG01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",907,"ΤΕΜ",1,"MC",1,"1FK22032AG010SA0"]
["1FK2203-2AG01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1216,"ΤΕΜ",1,"MC",1,"1FK22032AG011MA0"]
["1FK2203-2AG01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",907,"ΤΕΜ",1,"MC",1,"1FK22032AG011SA0"]
["1FK2203-2AG10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1377,"ΤΕΜ",1,"MC",1,"1FK22032AG100MA0"]
["1FK2203-2AG10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1069,"ΤΕΜ",1,"MC",1,"1FK22032AG100SA0"]
["1FK2203-2AG10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1377,"ΤΕΜ",1,"MC",1,"1FK22032AG101MA0"]
["1FK2203-2AG10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1069,"ΤΕΜ",1,"MC",1,"1FK22032AG101SA0"]
["1FK2203-2AG10-2MA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1377,"ΤΕΜ",1,"MC",1,"1FK22032AG102MA0"]
["1FK2203-2AG10-2SA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1069,"ΤΕΜ",1,"MC",1,"1FK22032AG102SA0"]
["1FK2203-2AG11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1463,"ΤΕΜ",1,"MC",1,"1FK22032AG110MA0"]
["1FK2203-2AG11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1155,"ΤΕΜ",1,"MC",1,"1FK22032AG110SA0"]
["1FK2203-2AG11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1463,"ΤΕΜ",1,"MC",1,"1FK22032AG111MA0"]
["1FK2203-2AG11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1155,"ΤΕΜ",1,"MC",1,"1FK22032AG111SA0"]
["1FK2203-4AG00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1253,"ΤΕΜ",1,"MC",1,"1FK22034AG000MA0"]
["1FK2203-4AG00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",944,"ΤΕΜ",1,"MC",1,"1FK22034AG000SA0"]
["1FK2203-4AG00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1253,"ΤΕΜ",1,"MC",1,"1FK22034AG001MA0"]
["1FK2203-4AG00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",944,"ΤΕΜ",1,"MC",1,"1FK22034AG001SA0"]
["1FK2203-4AG00-2MA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1253,"ΤΕΜ",1,"MC",1,"1FK22034AG002MA0"]
["1FK2203-4AG00-2SA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",944,"ΤΕΜ",1,"MC",1,"1FK22034AG002SA0"]
["1FK2203-4AG01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1339,"ΤΕΜ",1,"MC",1,"1FK22034AG010MA0"]
["1FK2203-4AG01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1030,"ΤΕΜ",1,"MC",1,"1FK22034AG010SA0"]
["1FK2203-4AG01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1339,"ΤΕΜ",1,"MC",1,"1FK22034AG011MA0"]
["1FK2203-4AG01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1030,"ΤΕΜ",1,"MC",1,"1FK22034AG011SA0"]
["1FK2203-4AG10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1500,"ΤΕΜ",1,"MC",1,"1FK22034AG100MA0"]
["1FK2203-4AG10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1192,"ΤΕΜ",1,"MC",1,"1FK22034AG100SA0"]
["1FK2203-4AG10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1500,"ΤΕΜ",1,"MC",1,"1FK22034AG101MA0"]
["1FK2203-4AG10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1192,"ΤΕΜ",1,"MC",1,"1FK22034AG101SA0"]
["1FK2203-4AG10-2MA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1500,"ΤΕΜ",1,"MC",1,"1FK22034AG102MA0"]
["1FK2203-4AG10-2SA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1192,"ΤΕΜ",1,"MC",1,"1FK22034AG102SA0"]
["1FK2203-4AG11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1587,"ΤΕΜ",1,"MC",1,"1FK22034AG110MA0"]
["1FK2203-4AG11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1278,"ΤΕΜ",1,"MC",1,"1FK22034AG110SA0"]
["1FK2203-4AG11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1587,"ΤΕΜ",1,"MC",1,"1FK22034AG111MA0"]
["1FK2203-4AG11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1278,"ΤΕΜ",1,"MC",1,"1FK22034AG111SA0"]
["1FK2204-5AF00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1355,"ΤΕΜ",1,"MC",1,"1FK22045AF000MA0"]
["1FK2204-5AF00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1355,"ΤΕΜ",1,"MC",1,"1FK22045AF000MB0"]
["1FK2204-5AF00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1047,"ΤΕΜ",1,"MC",1,"1FK22045AF000SA0"]
["1FK2204-5AF00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1047,"ΤΕΜ",1,"MC",1,"1FK22045AF000SB0"]
["1FK2204-5AF00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1355,"ΤΕΜ",1,"MC",1,"1FK22045AF001MA0"]
["1FK2204-5AF00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1355,"ΤΕΜ",1,"MC",1,"1FK22045AF001MB0"]
["1FK2204-5AF00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1047,"ΤΕΜ",1,"MC",1,"1FK22045AF001SA0"]
["1FK2204-5AF00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1047,"ΤΕΜ",1,"MC",1,"1FK22045AF001SB0"]
["1FK2204-5AF00-2MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1355,"ΤΕΜ",1,"MC",1,"1FK22045AF002MA0"]
["1FK2204-5AF00-2MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1355,"ΤΕΜ",1,"MC",1,"1FK22045AF002MB0"]
["1FK2204-5AF00-2SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1047,"ΤΕΜ",1,"MC",1,"1FK22045AF002SA0"]
["1FK2204-5AF00-2SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1047,"ΤΕΜ",1,"MC",1,"1FK22045AF002SB0"]
["1FK2204-5AF01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1442,"ΤΕΜ",1,"MC",1,"1FK22045AF010MA0"]
["1FK2204-5AF01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1442,"ΤΕΜ",1,"MC",1,"1FK22045AF010MB0"]
["1FK2204-5AF01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1133,"ΤΕΜ",1,"MC",1,"1FK22045AF010SA0"]
["1FK2204-5AF01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1133,"ΤΕΜ",1,"MC",1,"1FK22045AF010SB0"]
["1FK2204-5AF01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1442,"ΤΕΜ",1,"MC",1,"1FK22045AF011MA0"]
["1FK2204-5AF01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1442,"ΤΕΜ",1,"MC",1,"1FK22045AF011MB0"]
["1FK2204-5AF01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1133,"ΤΕΜ",1,"MC",1,"1FK22045AF011SA0"]
["1FK2204-5AF01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1133,"ΤΕΜ",1,"MC",1,"1FK22045AF011SB0"]
["1FK2204-5AF10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1603,"ΤΕΜ",1,"MC",1,"1FK22045AF100MA0"]
["1FK2204-5AF10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1603,"ΤΕΜ",1,"MC",1,"1FK22045AF100MB0"]
["1FK2204-5AF10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1294,"ΤΕΜ",1,"MC",1,"1FK22045AF100SA0"]
["1FK2204-5AF10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1294,"ΤΕΜ",1,"MC",1,"1FK22045AF100SB0"]
["1FK2204-5AF10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1603,"ΤΕΜ",1,"MC",1,"1FK22045AF101MA0"]
["1FK2204-5AF10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1603,"ΤΕΜ",1,"MC",1,"1FK22045AF101MB0"]
["1FK2204-5AF10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1294,"ΤΕΜ",1,"MC",1,"1FK22045AF101SA0"]
["1FK2204-5AF10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1294,"ΤΕΜ",1,"MC",1,"1FK22045AF101SB0"]
["1FK2204-5AF10-2MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1603,"ΤΕΜ",1,"MC",1,"1FK22045AF102MA0"]
["1FK2204-5AF10-2MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1603,"ΤΕΜ",1,"MC",1,"1FK22045AF102MB0"]
["1FK2204-5AF10-2SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1294,"ΤΕΜ",1,"MC",1,"1FK22045AF102SA0"]
["1FK2204-5AF10-2SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1294,"ΤΕΜ",1,"MC",1,"1FK22045AF102SB0"]
["1FK2204-5AF11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1689,"ΤΕΜ",1,"MC",1,"1FK22045AF110MA0"]
["1FK2204-5AF11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1689,"ΤΕΜ",1,"MC",1,"1FK22045AF110MB0"]
["1FK2204-5AF11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1380,"ΤΕΜ",1,"MC",1,"1FK22045AF110SA0"]
["1FK2204-5AF11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1380,"ΤΕΜ",1,"MC",1,"1FK22045AF110SB0"]
["1FK2204-5AF11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1689,"ΤΕΜ",1,"MC",1,"1FK22045AF111MA0"]
["1FK2204-5AF11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1689,"ΤΕΜ",1,"MC",1,"1FK22045AF111MB0"]
["1FK2204-5AF11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1380,"ΤΕΜ",1,"MC",1,"1FK22045AF111SA0"]
["1FK2204-5AF11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1380,"ΤΕΜ",1,"MC",1,"1FK22045AF111SB0"]
["1FK2204-5AK00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1355,"ΤΕΜ",1,"MC",1,"1FK22045AK000MA0"]
["1FK2204-5AK00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1355,"ΤΕΜ",1,"MC",1,"1FK22045AK000MB0"]
["1FK2204-5AK00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1047,"ΤΕΜ",1,"MC",1,"1FK22045AK000SA0"]
["1FK2204-5AK00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1047,"ΤΕΜ",1,"MC",1,"1FK22045AK000SB0"]
["1FK2204-5AK00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1355,"ΤΕΜ",1,"MC",1,"1FK22045AK001MA0"]
["1FK2204-5AK00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1355,"ΤΕΜ",1,"MC",1,"1FK22045AK001MB0"]
["1FK2204-5AK00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1047,"ΤΕΜ",1,"MC",1,"1FK22045AK001SA0"]
["1FK2204-5AK00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1047,"ΤΕΜ",1,"MC",1,"1FK22045AK001SB0"]
["1FK2204-5AK00-2MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1355,"ΤΕΜ",1,"MC",1,"1FK22045AK002MA0"]
["1FK2204-5AK00-2MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1355,"ΤΕΜ",1,"MC",1,"1FK22045AK002MB0"]
["1FK2204-5AK00-2SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1047,"ΤΕΜ",1,"MC",1,"1FK22045AK002SA0"]
["1FK2204-5AK00-2SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1047,"ΤΕΜ",1,"MC",1,"1FK22045AK002SB0"]
["1FK2204-5AK01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1442,"ΤΕΜ",1,"MC",1,"1FK22045AK010MA0"]
["1FK2204-5AK01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1442,"ΤΕΜ",1,"MC",1,"1FK22045AK010MB0"]
["1FK2204-5AK01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1133,"ΤΕΜ",1,"MC",1,"1FK22045AK010SA0"]
["1FK2204-5AK01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1133,"ΤΕΜ",1,"MC",1,"1FK22045AK010SB0"]
["1FK2204-5AK01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1442,"ΤΕΜ",1,"MC",1,"1FK22045AK011MA0"]
["1FK2204-5AK01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1442,"ΤΕΜ",1,"MC",1,"1FK22045AK011MB0"]
["1FK2204-5AK01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1133,"ΤΕΜ",1,"MC",1,"1FK22045AK011SA0"]
["1FK2204-5AK01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1133,"ΤΕΜ",1,"MC",1,"1FK22045AK011SB0"]
["1FK2204-5AK10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1603,"ΤΕΜ",1,"MC",1,"1FK22045AK100MA0"]
["1FK2204-5AK10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1603,"ΤΕΜ",1,"MC",1,"1FK22045AK100MB0"]
["1FK2204-5AK10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1294,"ΤΕΜ",1,"MC",1,"1FK22045AK100SA0"]
["1FK2204-5AK10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1294,"ΤΕΜ",1,"MC",1,"1FK22045AK100SB0"]
["1FK2204-5AK10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1603,"ΤΕΜ",1,"MC",1,"1FK22045AK101MA0"]
["1FK2204-5AK10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1603,"ΤΕΜ",1,"MC",1,"1FK22045AK101MB0"]
["1FK2204-5AK10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1294,"ΤΕΜ",1,"MC",1,"1FK22045AK101SA0"]
["1FK2204-5AK10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1294,"ΤΕΜ",1,"MC",1,"1FK22045AK101SB0"]
["1FK2204-5AK10-2MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1603,"ΤΕΜ",1,"MC",1,"1FK22045AK102MA0"]
["1FK2204-5AK10-2MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1603,"ΤΕΜ",1,"MC",1,"1FK22045AK102MB0"]
["1FK2204-5AK10-2SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1294,"ΤΕΜ",1,"MC",1,"1FK22045AK102SA0"]
["1FK2204-5AK10-2SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1294,"ΤΕΜ",1,"MC",1,"1FK22045AK102SB0"]
["1FK2204-5AK11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1689,"ΤΕΜ",1,"MC",1,"1FK22045AK110MA0"]
["1FK2204-5AK11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1689,"ΤΕΜ",1,"MC",1,"1FK22045AK110MB0"]
["1FK2204-5AK11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1380,"ΤΕΜ",1,"MC",1,"1FK22045AK110SA0"]
["1FK2204-5AK11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1380,"ΤΕΜ",1,"MC",1,"1FK22045AK110SB0"]
["1FK2204-5AK11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1689,"ΤΕΜ",1,"MC",1,"1FK22045AK111MA0"]
["1FK2204-5AK11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1689,"ΤΕΜ",1,"MC",1,"1FK22045AK111MB0"]
["1FK2204-5AK11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1380,"ΤΕΜ",1,"MC",1,"1FK22045AK111SA0"]
["1FK2204-5AK11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1380,"ΤΕΜ",1,"MC",1,"1FK22045AK111SB0"]
["1FK2204-6AF00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1417,"ΤΕΜ",1,"MC",1,"1FK22046AF000MA0"]
["1FK2204-6AF00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1417,"ΤΕΜ",1,"MC",1,"1FK22046AF000MB0"]
["1FK2204-6AF00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1108,"ΤΕΜ",1,"MC",1,"1FK22046AF000SA0"]
["1FK2204-6AF00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1108,"ΤΕΜ",1,"MC",1,"1FK22046AF000SB0"]
["1FK2204-6AF00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1417,"ΤΕΜ",1,"MC",1,"1FK22046AF001MA0"]
["1FK2204-6AF00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1417,"ΤΕΜ",1,"MC",1,"1FK22046AF001MB0"]
["1FK2204-6AF00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1108,"ΤΕΜ",1,"MC",1,"1FK22046AF001SA0"]
["1FK2204-6AF00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1108,"ΤΕΜ",1,"MC",1,"1FK22046AF001SB0"]
["1FK2204-6AF00-2MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1417,"ΤΕΜ",1,"MC",1,"1FK22046AF002MA0"]
["1FK2204-6AF00-2MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1417,"ΤΕΜ",1,"MC",1,"1FK22046AF002MB0"]
["1FK2204-6AF00-2SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1108,"ΤΕΜ",1,"MC",1,"1FK22046AF002SA0"]
["1FK2204-6AF00-2SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1108,"ΤΕΜ",1,"MC",1,"1FK22046AF002SB0"]
["1FK2204-6AF01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1503,"ΤΕΜ",1,"MC",1,"1FK22046AF010MA0"]
["1FK2204-6AF01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1503,"ΤΕΜ",1,"MC",1,"1FK22046AF010MB0"]
["1FK2204-6AF01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1195,"ΤΕΜ",1,"MC",1,"1FK22046AF010SA0"]
["1FK2204-6AF01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1195,"ΤΕΜ",1,"MC",1,"1FK22046AF010SB0"]
["1FK2204-6AF01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1503,"ΤΕΜ",1,"MC",1,"1FK22046AF011MA0"]
["1FK2204-6AF01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1503,"ΤΕΜ",1,"MC",1,"1FK22046AF011MB0"]
["1FK2204-6AF01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1195,"ΤΕΜ",1,"MC",1,"1FK22046AF011SA0"]
["1FK2204-6AF01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1195,"ΤΕΜ",1,"MC",1,"1FK22046AF011SB0"]
["1FK2204-6AF10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1664,"ΤΕΜ",1,"MC",1,"1FK22046AF100MA0"]
["1FK2204-6AF10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1664,"ΤΕΜ",1,"MC",1,"1FK22046AF100MB0"]
["1FK2204-6AF10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1356,"ΤΕΜ",1,"MC",1,"1FK22046AF100SA0"]
["1FK2204-6AF10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1356,"ΤΕΜ",1,"MC",1,"1FK22046AF100SB0"]
["1FK2204-6AF10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1664,"ΤΕΜ",1,"MC",1,"1FK22046AF101MA0"]
["1FK2204-6AF10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1664,"ΤΕΜ",1,"MC",1,"1FK22046AF101MB0"]
["1FK2204-6AF10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1356,"ΤΕΜ",1,"MC",1,"1FK22046AF101SA0"]
["1FK2204-6AF10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1356,"ΤΕΜ",1,"MC",1,"1FK22046AF101SB0"]
["1FK2204-6AF10-2MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1664,"ΤΕΜ",1,"MC",1,"1FK22046AF102MA0"]
["1FK2204-6AF10-2MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1664,"ΤΕΜ",1,"MC",1,"1FK22046AF102MB0"]
["1FK2204-6AF10-2SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1356,"ΤΕΜ",1,"MC",1,"1FK22046AF102SA0"]
["1FK2204-6AF10-2SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1356,"ΤΕΜ",1,"MC",1,"1FK22046AF102SB0"]
["1FK2204-6AF11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1751,"ΤΕΜ",1,"MC",1,"1FK22046AF110MA0"]
["1FK2204-6AF11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1751,"ΤΕΜ",1,"MC",1,"1FK22046AF110MB0"]
["1FK2204-6AF11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1442,"ΤΕΜ",1,"MC",1,"1FK22046AF110SA0"]
["1FK2204-6AF11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1442,"ΤΕΜ",1,"MC",1,"1FK22046AF110SB0"]
["1FK2204-6AF11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1751,"ΤΕΜ",1,"MC",1,"1FK22046AF111MA0"]
["1FK2204-6AF11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1751,"ΤΕΜ",1,"MC",1,"1FK22046AF111MB0"]
["1FK2204-6AF11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1442,"ΤΕΜ",1,"MC",1,"1FK22046AF111SA0"]
["1FK2204-6AF11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1442,"ΤΕΜ",1,"MC",1,"1FK22046AF111SB0"]
["1FK2205-2AF00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1439,"ΤΕΜ",1,"MC",1,"1FK22052AF000MA0"]
["1FK2205-2AF00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1439,"ΤΕΜ",1,"MC",1,"1FK22052AF000MB0"]
["1FK2205-2AF00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1130,"ΤΕΜ",1,"MC",1,"1FK22052AF000SA0"]
["1FK2205-2AF00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1130,"ΤΕΜ",1,"MC",1,"1FK22052AF000SB0"]
["1FK2205-2AF00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1439,"ΤΕΜ",1,"MC",1,"1FK22052AF001MA0"]
["1FK2205-2AF00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1439,"ΤΕΜ",1,"MC",1,"1FK22052AF001MB0"]
["1FK2205-2AF00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1130,"ΤΕΜ",1,"MC",1,"1FK22052AF001SA0"]
["1FK2205-2AF00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1130,"ΤΕΜ",1,"MC",1,"1FK22052AF001SB0"]
["1FK2205-2AF01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1525,"ΤΕΜ",1,"MC",1,"1FK22052AF010MA0"]
["1FK2205-2AF01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1525,"ΤΕΜ",1,"MC",1,"1FK22052AF010MB0"]
["1FK2205-2AF01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1217,"ΤΕΜ",1,"MC",1,"1FK22052AF010SA0"]
["1FK2205-2AF01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1217,"ΤΕΜ",1,"MC",1,"1FK22052AF010SB0"]
["1FK2205-2AF01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1525,"ΤΕΜ",1,"MC",1,"1FK22052AF011MA0"]
["1FK2205-2AF01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1525,"ΤΕΜ",1,"MC",1,"1FK22052AF011MB0"]
["1FK2205-2AF01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1217,"ΤΕΜ",1,"MC",1,"1FK22052AF011SA0"]
["1FK2205-2AF01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1217,"ΤΕΜ",1,"MC",1,"1FK22052AF011SB0"]
["1FK2205-2AF10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1728,"ΤΕΜ",1,"MC",1,"1FK22052AF100MA0"]
["1FK2205-2AF10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1728,"ΤΕΜ",1,"MC",1,"1FK22052AF100MB0"]
["1FK2205-2AF10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1419,"ΤΕΜ",1,"MC",1,"1FK22052AF100SA0"]
["1FK2205-2AF10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1419,"ΤΕΜ",1,"MC",1,"1FK22052AF100SB0"]
["1FK2205-2AF10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1728,"ΤΕΜ",1,"MC",1,"1FK22052AF101MA0"]
["1FK2205-2AF10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1728,"ΤΕΜ",1,"MC",1,"1FK22052AF101MB0"]
["1FK2205-2AF10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1419,"ΤΕΜ",1,"MC",1,"1FK22052AF101SA0"]
["1FK2205-2AF10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1419,"ΤΕΜ",1,"MC",1,"1FK22052AF101SB0"]
["1FK2205-2AF11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1814,"ΤΕΜ",1,"MC",1,"1FK22052AF110MA0"]
["1FK2205-2AF11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1814,"ΤΕΜ",1,"MC",1,"1FK22052AF110MB0"]
["1FK2205-2AF11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1505,"ΤΕΜ",1,"MC",1,"1FK22052AF110SA0"]
["1FK2205-2AF11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1505,"ΤΕΜ",1,"MC",1,"1FK22052AF110SB0"]
["1FK2205-2AF11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1814,"ΤΕΜ",1,"MC",1,"1FK22052AF111MA0"]
["1FK2205-2AF11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1814,"ΤΕΜ",1,"MC",1,"1FK22052AF111MB0"]
["1FK2205-2AF11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1505,"ΤΕΜ",1,"MC",1,"1FK22052AF111SA0"]
["1FK2205-2AF11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1505,"ΤΕΜ",1,"MC",1,"1FK22052AF111SB0"]
["1FK2205-4AF00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1643,"ΤΕΜ",1,"MC",1,"1FK22054AF000MA0"]
["1FK2205-4AF00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1643,"ΤΕΜ",1,"MC",1,"1FK22054AF000MB0"]
["1FK2205-4AF00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1334,"ΤΕΜ",1,"MC",1,"1FK22054AF000SA0"]
["1FK2205-4AF00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1334,"ΤΕΜ",1,"MC",1,"1FK22054AF000SB0"]
["1FK2205-4AF00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1643,"ΤΕΜ",1,"MC",1,"1FK22054AF001MA0"]
["1FK2205-4AF00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1643,"ΤΕΜ",1,"MC",1,"1FK22054AF001MB0"]
["1FK2205-4AF00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1334,"ΤΕΜ",1,"MC",1,"1FK22054AF001SA0"]
["1FK2205-4AF00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1334,"ΤΕΜ",1,"MC",1,"1FK22054AF001SB0"]
["1FK2205-4AF01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1729,"ΤΕΜ",1,"MC",1,"1FK22054AF010MA0"]
["1FK2205-4AF01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1729,"ΤΕΜ",1,"MC",1,"1FK22054AF010MB0"]
["1FK2205-4AF01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1420,"ΤΕΜ",1,"MC",1,"1FK22054AF010SA0"]
["1FK2205-4AF01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1420,"ΤΕΜ",1,"MC",1,"1FK22054AF010SB0"]
["1FK2205-4AF01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1729,"ΤΕΜ",1,"MC",1,"1FK22054AF011MA0"]
["1FK2205-4AF01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1729,"ΤΕΜ",1,"MC",1,"1FK22054AF011MB0"]
["1FK2205-4AF01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1420,"ΤΕΜ",1,"MC",1,"1FK22054AF011SA0"]
["1FK2205-4AF01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1420,"ΤΕΜ",1,"MC",1,"1FK22054AF011SB0"]
["1FK2205-4AF10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1931,"ΤΕΜ",1,"MC",1,"1FK22054AF100MA0"]
["1FK2205-4AF10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1931,"ΤΕΜ",1,"MC",1,"1FK22054AF100MB0"]
["1FK2205-4AF10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1623,"ΤΕΜ",1,"MC",1,"1FK22054AF100SA0"]
["1FK2205-4AF10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1623,"ΤΕΜ",1,"MC",1,"1FK22054AF100SB0"]
["1FK2205-4AF10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1931,"ΤΕΜ",1,"MC",1,"1FK22054AF101MA0"]
["1FK2205-4AF10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1931,"ΤΕΜ",1,"MC",1,"1FK22054AF101MB0"]
["1FK2205-4AF10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1623,"ΤΕΜ",1,"MC",1,"1FK22054AF101SA0"]
["1FK2205-4AF10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1623,"ΤΕΜ",1,"MC",1,"1FK22054AF101SB0"]
["1FK2205-4AF11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",2018,"ΤΕΜ",1,"MC",1,"1FK22054AF110MA0"]
["1FK2205-4AF11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",2018,"ΤΕΜ",1,"MC",1,"1FK22054AF110MB0"]
["1FK2205-4AF11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1709,"ΤΕΜ",1,"MC",1,"1FK22054AF110SA0"]
["1FK2205-4AF11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1709,"ΤΕΜ",1,"MC",1,"1FK22054AF110SB0"]
["1FK2205-4AF11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",2018,"ΤΕΜ",1,"MC",1,"1FK22054AF111MA0"]
["1FK2205-4AF11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",2018,"ΤΕΜ",1,"MC",1,"1FK22054AF111MB0"]
["1FK2205-4AF11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1709,"ΤΕΜ",1,"MC",1,"1FK22054AF111SA0"]
["1FK2205-4AF11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1709,"ΤΕΜ",1,"MC",1,"1FK22054AF111SB0"]
["1FK2206-2AF00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",1680,"ΤΕΜ",1,"MC",1,"1FK22062AF000MA0"]
["1FK2206-2AF00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1680,"ΤΕΜ",1,"MC",1,"1FK22062AF000MB0"]
["1FK2206-2AF00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1372,"ΤΕΜ",1,"MC",1,"1FK22062AF000SA0"]
["1FK2206-2AF00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1372,"ΤΕΜ",1,"MC",1,"1FK22062AF000SB0"]
["1FK2206-2AF00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",1680,"ΤΕΜ",1,"MC",1,"1FK22062AF001MA0"]
["1FK2206-2AF00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1680,"ΤΕΜ",1,"MC",1,"1FK22062AF001MB0"]
["1FK2206-2AF00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1372,"ΤΕΜ",1,"MC",1,"1FK22062AF001SA0"]
["1FK2206-2AF00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1372,"ΤΕΜ",1,"MC",1,"1FK22062AF001SB0"]
["1FK2206-2AF01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",1766,"ΤΕΜ",1,"MC",1,"1FK22062AF010MA0"]
["1FK2206-2AF01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1766,"ΤΕΜ",1,"MC",1,"1FK22062AF010MB0"]
["1FK2206-2AF01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1458,"ΤΕΜ",1,"MC",1,"1FK22062AF010SA0"]
["1FK2206-2AF01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1458,"ΤΕΜ",1,"MC",1,"1FK22062AF010SB0"]
["1FK2206-2AF01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",1766,"ΤΕΜ",1,"MC",1,"1FK22062AF011MA0"]
["1FK2206-2AF01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1766,"ΤΕΜ",1,"MC",1,"1FK22062AF011MB0"]
["1FK2206-2AF01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1458,"ΤΕΜ",1,"MC",1,"1FK22062AF011SA0"]
["1FK2206-2AF01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1458,"ΤΕΜ",1,"MC",1,"1FK22062AF011SB0"]
["1FK2206-2AF10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2010,"ΤΕΜ",1,"MC",1,"1FK22062AF100MA0"]
["1FK2206-2AF10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2010,"ΤΕΜ",1,"MC",1,"1FK22062AF100MB0"]
["1FK2206-2AF10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1702,"ΤΕΜ",1,"MC",1,"1FK22062AF100SA0"]
["1FK2206-2AF10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1702,"ΤΕΜ",1,"MC",1,"1FK22062AF100SB0"]
["1FK2206-2AF10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2010,"ΤΕΜ",1,"MC",1,"1FK22062AF101MA0"]
["1FK2206-2AF10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2010,"ΤΕΜ",1,"MC",1,"1FK22062AF101MB0"]
["1FK2206-2AF10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1702,"ΤΕΜ",1,"MC",1,"1FK22062AF101SA0"]
["1FK2206-2AF10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1702,"ΤΕΜ",1,"MC",1,"1FK22062AF101SB0"]
["1FK2206-2AF11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2096,"ΤΕΜ",1,"MC",1,"1FK22062AF110MA0"]
["1FK2206-2AF11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2096,"ΤΕΜ",1,"MC",1,"1FK22062AF110MB0"]
["1FK2206-2AF11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1788,"ΤΕΜ",1,"MC",1,"1FK22062AF110SA0"]
["1FK2206-2AF11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1788,"ΤΕΜ",1,"MC",1,"1FK22062AF110SB0"]
["1FK2206-2AF11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2096,"ΤΕΜ",1,"MC",1,"1FK22062AF111MA0"]
["1FK2206-2AF11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2096,"ΤΕΜ",1,"MC",1,"1FK22062AF111MB0"]
["1FK2206-2AF11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1788,"ΤΕΜ",1,"MC",1,"1FK22062AF111SA0"]
["1FK2206-2AF11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1788,"ΤΕΜ",1,"MC",1,"1FK22062AF111SB0"]
["1FK2206-4AF00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2094,"ΤΕΜ",1,"MC",1,"1FK22064AF000MA0"]
["1FK2206-4AF00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2094,"ΤΕΜ",1,"MC",1,"1FK22064AF000MB0"]
["1FK2206-4AF00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1785,"ΤΕΜ",1,"MC",1,"1FK22064AF000SA0"]
["1FK2206-4AF00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1785,"ΤΕΜ",1,"MC",1,"1FK22064AF000SB0"]
["1FK2206-4AF00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2094,"ΤΕΜ",1,"MC",1,"1FK22064AF001MA0"]
["1FK2206-4AF00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2094,"ΤΕΜ",1,"MC",1,"1FK22064AF001MB0"]
["1FK2206-4AF00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1785,"ΤΕΜ",1,"MC",1,"1FK22064AF001SA0"]
["1FK2206-4AF00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1785,"ΤΕΜ",1,"MC",1,"1FK22064AF001SB0"]
["1FK2206-4AF01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2180,"ΤΕΜ",1,"MC",1,"1FK22064AF010MA0"]
["1FK2206-4AF01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2180,"ΤΕΜ",1,"MC",1,"1FK22064AF010MB0"]
["1FK2206-4AF01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1871,"ΤΕΜ",1,"MC",1,"1FK22064AF010SA0"]
["1FK2206-4AF01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1871,"ΤΕΜ",1,"MC",1,"1FK22064AF010SB0"]
["1FK2206-4AF01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2180,"ΤΕΜ",1,"MC",1,"1FK22064AF011MA0"]
["1FK2206-4AF01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2180,"ΤΕΜ",1,"MC",1,"1FK22064AF011MB0"]
["1FK2206-4AF01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1871,"ΤΕΜ",1,"MC",1,"1FK22064AF011SA0"]
["1FK2206-4AF01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1871,"ΤΕΜ",1,"MC",1,"1FK22064AF011SB0"]
["1FK2206-4AF10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2424,"ΤΕΜ",1,"MC",1,"1FK22064AF100MA0"]
["1FK2206-4AF10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2424,"ΤΕΜ",1,"MC",1,"1FK22064AF100MB0"]
["1FK2206-4AF10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2115,"ΤΕΜ",1,"MC",1,"1FK22064AF100SA0"]
["1FK2206-4AF10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2115,"ΤΕΜ",1,"MC",1,"1FK22064AF100SB0"]
["1FK2206-4AF10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2424,"ΤΕΜ",1,"MC",1,"1FK22064AF101MA0"]
["1FK2206-4AF10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2424,"ΤΕΜ",1,"MC",1,"1FK22064AF101MB0"]
["1FK2206-4AF10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2115,"ΤΕΜ",1,"MC",1,"1FK22064AF101SA0"]
["1FK2206-4AF10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2115,"ΤΕΜ",1,"MC",1,"1FK22064AF101SB0"]
["1FK2206-4AF11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2510,"ΤΕΜ",1,"MC",1,"1FK22064AF110MA0"]
["1FK2206-4AF11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2510,"ΤΕΜ",1,"MC",1,"1FK22064AF110MB0"]
["1FK2206-4AF11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2201,"ΤΕΜ",1,"MC",1,"1FK22064AF110SA0"]
["1FK2206-4AF11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2201,"ΤΕΜ",1,"MC",1,"1FK22064AF110SB0"]
["1FK2206-4AF11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2510,"ΤΕΜ",1,"MC",1,"1FK22064AF111MA0"]
["1FK2206-4AF11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2510,"ΤΕΜ",1,"MC",1,"1FK22064AF111MB0"]
["1FK2206-4AF11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2201,"ΤΕΜ",1,"MC",1,"1FK22064AF111SA0"]
["1FK2206-4AF11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2201,"ΤΕΜ",1,"MC",1,"1FK22064AF111SB0"]
["1FK2208-3AC00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2454,"ΤΕΜ",1,"MC",1,"1FK22083AC000MA0"]
["1FK2208-3AC00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2454,"ΤΕΜ",1,"MC",1,"1FK22083AC000MB0"]
["1FK2208-3AC00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2146,"ΤΕΜ",1,"MC",1,"1FK22083AC000SA0"]
["1FK2208-3AC00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2146,"ΤΕΜ",1,"MC",1,"1FK22083AC000SB0"]
["1FK2208-3AC00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2454,"ΤΕΜ",1,"MC",1,"1FK22083AC001MA0"]
["1FK2208-3AC00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2454,"ΤΕΜ",1,"MC",1,"1FK22083AC001MB0"]
["1FK2208-3AC00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2146,"ΤΕΜ",1,"MC",1,"1FK22083AC001SA0"]
["1FK2208-3AC00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2146,"ΤΕΜ",1,"MC",1,"1FK22083AC001SB0"]
["1FK2208-3AC01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2540,"ΤΕΜ",1,"MC",1,"1FK22083AC010MA0"]
["1FK2208-3AC01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2540,"ΤΕΜ",1,"MC",1,"1FK22083AC010MB0"]
["1FK2208-3AC01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2232,"ΤΕΜ",1,"MC",1,"1FK22083AC010SA0"]
["1FK2208-3AC01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2232,"ΤΕΜ",1,"MC",1,"1FK22083AC010SB0"]
["1FK2208-3AC01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2540,"ΤΕΜ",1,"MC",1,"1FK22083AC011MA0"]
["1FK2208-3AC01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2540,"ΤΕΜ",1,"MC",1,"1FK22083AC011MB0"]
["1FK2208-3AC01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2232,"ΤΕΜ",1,"MC",1,"1FK22083AC011SA0"]
["1FK2208-3AC01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2232,"ΤΕΜ",1,"MC",1,"1FK22083AC011SB0"]
["1FK2208-3AC10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2867,"ΤΕΜ",1,"MC",1,"1FK22083AC100MA0"]
["1FK2208-3AC10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2867,"ΤΕΜ",1,"MC",1,"1FK22083AC100MB0"]
["1FK2208-3AC10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2558,"ΤΕΜ",1,"MC",1,"1FK22083AC100SA0"]
["1FK2208-3AC10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2558,"ΤΕΜ",1,"MC",1,"1FK22083AC100SB0"]
["1FK2208-3AC10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2867,"ΤΕΜ",1,"MC",1,"1FK22083AC101MA0"]
["1FK2208-3AC10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2867,"ΤΕΜ",1,"MC",1,"1FK22083AC101MB0"]
["1FK2208-3AC10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2558,"ΤΕΜ",1,"MC",1,"1FK22083AC101SA0"]
["1FK2208-3AC10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2558,"ΤΕΜ",1,"MC",1,"1FK22083AC101SB0"]
["1FK2208-3AC11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2953,"ΤΕΜ",1,"MC",1,"1FK22083AC110MA0"]
["1FK2208-3AC11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2953,"ΤΕΜ",1,"MC",1,"1FK22083AC110MB0"]
["1FK2208-3AC11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2644,"ΤΕΜ",1,"MC",1,"1FK22083AC110SA0"]
["1FK2208-3AC11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2644,"ΤΕΜ",1,"MC",1,"1FK22083AC110SB0"]
["1FK2208-3AC11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2953,"ΤΕΜ",1,"MC",1,"1FK22083AC111MA0"]
["1FK2208-3AC11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2953,"ΤΕΜ",1,"MC",1,"1FK22083AC111MB0"]
["1FK2208-3AC11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2644,"ΤΕΜ",1,"MC",1,"1FK22083AC111SA0"]
["1FK2208-3AC11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2644,"ΤΕΜ",1,"MC",1,"1FK22083AC111SB0"]
["1FK2208-4AC00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2700,"ΤΕΜ",1,"MC",1,"1FK22084AC000MA0"]
["1FK2208-4AC00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2700,"ΤΕΜ",1,"MC",1,"1FK22084AC000MB0"]
["1FK2208-4AC00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2391,"ΤΕΜ",1,"MC",1,"1FK22084AC000SA0"]
["1FK2208-4AC00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2391,"ΤΕΜ",1,"MC",1,"1FK22084AC000SB0"]
["1FK2208-4AC00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2700,"ΤΕΜ",1,"MC",1,"1FK22084AC001MA0"]
["1FK2208-4AC00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2700,"ΤΕΜ",1,"MC",1,"1FK22084AC001MB0"]
["1FK2208-4AC00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2391,"ΤΕΜ",1,"MC",1,"1FK22084AC001SA0"]
["1FK2208-4AC00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2391,"ΤΕΜ",1,"MC",1,"1FK22084AC001SB0"]
["1FK2208-4AC01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2786,"ΤΕΜ",1,"MC",1,"1FK22084AC010MA0"]
["1FK2208-4AC01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2786,"ΤΕΜ",1,"MC",1,"1FK22084AC010MB0"]
["1FK2208-4AC01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2477,"ΤΕΜ",1,"MC",1,"1FK22084AC010SA0"]
["1FK2208-4AC01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2477,"ΤΕΜ",1,"MC",1,"1FK22084AC010SB0"]
["1FK2208-4AC01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2786,"ΤΕΜ",1,"MC",1,"1FK22084AC011MA0"]
["1FK2208-4AC01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2786,"ΤΕΜ",1,"MC",1,"1FK22084AC011MB0"]
["1FK2208-4AC01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2477,"ΤΕΜ",1,"MC",1,"1FK22084AC011SA0"]
["1FK2208-4AC01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2477,"ΤΕΜ",1,"MC",1,"1FK22084AC011SB0"]
["1FK2208-4AC10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3112,"ΤΕΜ",1,"MC",1,"1FK22084AC100MA0"]
["1FK2208-4AC10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3112,"ΤΕΜ",1,"MC",1,"1FK22084AC100MB0"]
["1FK2208-4AC10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2803,"ΤΕΜ",1,"MC",1,"1FK22084AC100SA0"]
["1FK2208-4AC10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2803,"ΤΕΜ",1,"MC",1,"1FK22084AC100SB0"]
["1FK2208-4AC10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3112,"ΤΕΜ",1,"MC",1,"1FK22084AC101MA0"]
["1FK2208-4AC10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3112,"ΤΕΜ",1,"MC",1,"1FK22084AC101MB0"]
["1FK2208-4AC10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2803,"ΤΕΜ",1,"MC",1,"1FK22084AC101SA0"]
["1FK2208-4AC10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2803,"ΤΕΜ",1,"MC",1,"1FK22084AC101SB0"]
["1FK2208-4AC11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3198,"ΤΕΜ",1,"MC",1,"1FK22084AC110MA0"]
["1FK2208-4AC11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3198,"ΤΕΜ",1,"MC",1,"1FK22084AC110MB0"]
["1FK2208-4AC11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2890,"ΤΕΜ",1,"MC",1,"1FK22084AC110SA0"]
["1FK2208-4AC11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2890,"ΤΕΜ",1,"MC",1,"1FK22084AC110SB0"]
["1FK2208-4AC11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3198,"ΤΕΜ",1,"MC",1,"1FK22084AC111MA0"]
["1FK2208-4AC11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3198,"ΤΕΜ",1,"MC",1,"1FK22084AC111MB0"]
["1FK2208-4AC11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2890,"ΤΕΜ",1,"MC",1,"1FK22084AC111SA0"]
["1FK2208-4AC11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2890,"ΤΕΜ",1,"MC",1,"1FK22084AC111SB0"]
["1FK2208-5AC00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3009,"ΤΕΜ",1,"MC",1,"1FK22085AC000MA0"]
["1FK2208-5AC00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3009,"ΤΕΜ",1,"MC",1,"1FK22085AC000MB0"]
["1FK2208-5AC00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2700,"ΤΕΜ",1,"MC",1,"1FK22085AC000SA0"]
["1FK2208-5AC00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2700,"ΤΕΜ",1,"MC",1,"1FK22085AC000SB0"]
["1FK2208-5AC00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3009,"ΤΕΜ",1,"MC",1,"1FK22085AC001MA0"]
["1FK2208-5AC00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3009,"ΤΕΜ",1,"MC",1,"1FK22085AC001MB0"]
["1FK2208-5AC00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2700,"ΤΕΜ",1,"MC",1,"1FK22085AC001SA0"]
["1FK2208-5AC00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2700,"ΤΕΜ",1,"MC",1,"1FK22085AC001SB0"]
["1FK2208-5AC01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3095,"ΤΕΜ",1,"MC",1,"1FK22085AC010MA0"]
["1FK2208-5AC01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3095,"ΤΕΜ",1,"MC",1,"1FK22085AC010MB0"]
["1FK2208-5AC01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2786,"ΤΕΜ",1,"MC",1,"1FK22085AC010SA0"]
["1FK2208-5AC01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2786,"ΤΕΜ",1,"MC",1,"1FK22085AC010SB0"]
["1FK2208-5AC01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3095,"ΤΕΜ",1,"MC",1,"1FK22085AC011MA0"]
["1FK2208-5AC01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3095,"ΤΕΜ",1,"MC",1,"1FK22085AC011MB0"]
["1FK2208-5AC01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2786,"ΤΕΜ",1,"MC",1,"1FK22085AC011SA0"]
["1FK2208-5AC01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2786,"ΤΕΜ",1,"MC",1,"1FK22085AC011SB0"]
["1FK2208-5AC10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3421,"ΤΕΜ",1,"MC",1,"1FK22085AC100MA0"]
["1FK2208-5AC10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3421,"ΤΕΜ",1,"MC",1,"1FK22085AC100MB0"]
["1FK2208-5AC10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3112,"ΤΕΜ",1,"MC",1,"1FK22085AC100SA0"]
["1FK2208-5AC10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3112,"ΤΕΜ",1,"MC",1,"1FK22085AC100SB0"]
["1FK2208-5AC10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3421,"ΤΕΜ",1,"MC",1,"1FK22085AC101MA0"]
["1FK2208-5AC10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3421,"ΤΕΜ",1,"MC",1,"1FK22085AC101MB0"]
["1FK2208-5AC10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3112,"ΤΕΜ",1,"MC",1,"1FK22085AC101SA0"]
["1FK2208-5AC10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3112,"ΤΕΜ",1,"MC",1,"1FK22085AC101SB0"]
["1FK2208-5AC11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3507,"ΤΕΜ",1,"MC",1,"1FK22085AC110MA0"]
["1FK2208-5AC11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3507,"ΤΕΜ",1,"MC",1,"1FK22085AC110MB0"]
["1FK2208-5AC11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3198,"ΤΕΜ",1,"MC",1,"1FK22085AC110SA0"]
["1FK2208-5AC11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3198,"ΤΕΜ",1,"MC",1,"1FK22085AC110SB0"]
["1FK2208-5AC11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3507,"ΤΕΜ",1,"MC",1,"1FK22085AC111MA0"]
["1FK2208-5AC11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3507,"ΤΕΜ",1,"MC",1,"1FK22085AC111MB0"]
["1FK2208-5AC11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3198,"ΤΕΜ",1,"MC",1,"1FK22085AC111SA0"]
["1FK2208-5AC11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3198,"ΤΕΜ",1,"MC",1,"1FK22085AC111SB0"]
["1FK2210-3AB00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3173,"ΤΕΜ",1,"MC",1,"1FK22103AB000MA0"]
["1FK2210-3AB00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3173,"ΤΕΜ",1,"MC",1,"1FK22103AB000MB0"]
["1FK2210-3AB00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2864,"ΤΕΜ",1,"MC",1,"1FK22103AB000SA0"]
["1FK2210-3AB00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2864,"ΤΕΜ",1,"MC",1,"1FK22103AB000SB0"]
["1FK2210-3AB00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3173,"ΤΕΜ",1,"MC",1,"1FK22103AB001MA0"]
["1FK2210-3AB00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3173,"ΤΕΜ",1,"MC",1,"1FK22103AB001MB0"]
["1FK2210-3AB00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2864,"ΤΕΜ",1,"MC",1,"1FK22103AB001SA0"]
["1FK2210-3AB00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2864,"ΤΕΜ",1,"MC",1,"1FK22103AB001SB0"]
["1FK2210-3AB01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3259,"ΤΕΜ",1,"MC",1,"1FK22103AB010MA0"]
["1FK2210-3AB01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3259,"ΤΕΜ",1,"MC",1,"1FK22103AB010MB0"]
["1FK2210-3AB01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2951,"ΤΕΜ",1,"MC",1,"1FK22103AB010SA0"]
["1FK2210-3AB01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2951,"ΤΕΜ",1,"MC",1,"1FK22103AB010SB0"]
["1FK2210-3AB01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3259,"ΤΕΜ",1,"MC",1,"1FK22103AB011MA0"]
["1FK2210-3AB01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3259,"ΤΕΜ",1,"MC",1,"1FK22103AB011MB0"]
["1FK2210-3AB01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2951,"ΤΕΜ",1,"MC",1,"1FK22103AB011SA0"]
["1FK2210-3AB01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2951,"ΤΕΜ",1,"MC",1,"1FK22103AB011SB0"]
["1FK2210-3AB10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3627,"ΤΕΜ",1,"MC",1,"1FK22103AB100MA0"]
["1FK2210-3AB10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3627,"ΤΕΜ",1,"MC",1,"1FK22103AB100MB0"]
["1FK2210-3AB10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3318,"ΤΕΜ",1,"MC",1,"1FK22103AB100SA0"]
["1FK2210-3AB10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3318,"ΤΕΜ",1,"MC",1,"1FK22103AB100SB0"]
["1FK2210-3AB10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3627,"ΤΕΜ",1,"MC",1,"1FK22103AB101MA0"]
["1FK2210-3AB10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3627,"ΤΕΜ",1,"MC",1,"1FK22103AB101MB0"]
["1FK2210-3AB10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3318,"ΤΕΜ",1,"MC",1,"1FK22103AB101SA0"]
["1FK2210-3AB10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3318,"ΤΕΜ",1,"MC",1,"1FK22103AB101SB0"]
["1FK2210-3AB11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3713,"ΤΕΜ",1,"MC",1,"1FK22103AB110MA0"]
["1FK2210-3AB11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3713,"ΤΕΜ",1,"MC",1,"1FK22103AB110MB0"]
["1FK2210-3AB11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3404,"ΤΕΜ",1,"MC",1,"1FK22103AB110SA0"]
["1FK2210-3AB11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3404,"ΤΕΜ",1,"MC",1,"1FK22103AB110SB0"]
["1FK2210-3AB11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3713,"ΤΕΜ",1,"MC",1,"1FK22103AB111MA0"]
["1FK2210-3AB11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3713,"ΤΕΜ",1,"MC",1,"1FK22103AB111MB0"]
["1FK2210-3AB11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3404,"ΤΕΜ",1,"MC",1,"1FK22103AB111SA0"]
["1FK2210-3AB11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3404,"ΤΕΜ",1,"MC",1,"1FK22103AB111SB0"]
["1FK2210-3AC00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3173,"ΤΕΜ",1,"MC",1,"1FK22103AC000MA0"]
["1FK2210-3AC00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3173,"ΤΕΜ",1,"MC",1,"1FK22103AC000MB0"]
["1FK2210-3AC00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2864,"ΤΕΜ",1,"MC",1,"1FK22103AC000SA0"]
["1FK2210-3AC00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2864,"ΤΕΜ",1,"MC",1,"1FK22103AC000SB0"]
["1FK2210-3AC00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3173,"ΤΕΜ",1,"MC",1,"1FK22103AC001MA0"]
["1FK2210-3AC00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3173,"ΤΕΜ",1,"MC",1,"1FK22103AC001MB0"]
["1FK2210-3AC00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2864,"ΤΕΜ",1,"MC",1,"1FK22103AC001SA0"]
["1FK2210-3AC00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2864,"ΤΕΜ",1,"MC",1,"1FK22103AC001SB0"]
["1FK2210-3AC01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3259,"ΤΕΜ",1,"MC",1,"1FK22103AC010MA0"]
["1FK2210-3AC01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3259,"ΤΕΜ",1,"MC",1,"1FK22103AC010MB0"]
["1FK2210-3AC01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2951,"ΤΕΜ",1,"MC",1,"1FK22103AC010SA0"]
["1FK2210-3AC01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2951,"ΤΕΜ",1,"MC",1,"1FK22103AC010SB0"]
["1FK2210-3AC01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3259,"ΤΕΜ",1,"MC",1,"1FK22103AC011MA0"]
["1FK2210-3AC01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3259,"ΤΕΜ",1,"MC",1,"1FK22103AC011MB0"]
["1FK2210-3AC01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2951,"ΤΕΜ",1,"MC",1,"1FK22103AC011SA0"]
["1FK2210-3AC01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2951,"ΤΕΜ",1,"MC",1,"1FK22103AC011SB0"]
["1FK2210-3AC10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3627,"ΤΕΜ",1,"MC",1,"1FK22103AC100MA0"]
["1FK2210-3AC10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3627,"ΤΕΜ",1,"MC",1,"1FK22103AC100MB0"]
["1FK2210-3AC10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3318,"ΤΕΜ",1,"MC",1,"1FK22103AC100SA0"]
["1FK2210-3AC10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3318,"ΤΕΜ",1,"MC",1,"1FK22103AC100SB0"]
["1FK2210-3AC10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3627,"ΤΕΜ",1,"MC",1,"1FK22103AC101MA0"]
["1FK2210-3AC10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3627,"ΤΕΜ",1,"MC",1,"1FK22103AC101MB0"]
["1FK2210-3AC10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3318,"ΤΕΜ",1,"MC",1,"1FK22103AC101SA0"]
["1FK2210-3AC10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3318,"ΤΕΜ",1,"MC",1,"1FK22103AC101SB0"]
["1FK2210-3AC11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3713,"ΤΕΜ",1,"MC",1,"1FK22103AC110MA0"]
["1FK2210-3AC11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3713,"ΤΕΜ",1,"MC",1,"1FK22103AC110MB0"]
["1FK2210-3AC11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3404,"ΤΕΜ",1,"MC",1,"1FK22103AC110SA0"]
["1FK2210-3AC11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3404,"ΤΕΜ",1,"MC",1,"1FK22103AC110SB0"]
["1FK2210-3AC11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3713,"ΤΕΜ",1,"MC",1,"1FK22103AC111MA0"]
["1FK2210-3AC11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3713,"ΤΕΜ",1,"MC",1,"1FK22103AC111MB0"]
["1FK2210-3AC11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3404,"ΤΕΜ",1,"MC",1,"1FK22103AC111SA0"]
["1FK2210-3AC11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3404,"ΤΕΜ",1,"MC",1,"1FK22103AC111SB0"]
["1FK2210-4AB00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3815,"ΤΕΜ",1,"MC",1,"1FK22104AB000MA0"]
["1FK2210-4AB00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3815,"ΤΕΜ",1,"MC",1,"1FK22104AB000MB0"]
["1FK2210-4AB00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3507,"ΤΕΜ",1,"MC",1,"1FK22104AB000SA0"]
["1FK2210-4AB00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3507,"ΤΕΜ",1,"MC",1,"1FK22104AB000SB0"]
["1FK2210-4AB00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3815,"ΤΕΜ",1,"MC",1,"1FK22104AB001MA0"]
["1FK2210-4AB00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3815,"ΤΕΜ",1,"MC",1,"1FK22104AB001MB0"]
["1FK2210-4AB00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3507,"ΤΕΜ",1,"MC",1,"1FK22104AB001SA0"]
["1FK2210-4AB00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3507,"ΤΕΜ",1,"MC",1,"1FK22104AB001SB0"]
["1FK2210-4AB01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3902,"ΤΕΜ",1,"MC",1,"1FK22104AB010MA0"]
["1FK2210-4AB01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3902,"ΤΕΜ",1,"MC",1,"1FK22104AB010MB0"]
["1FK2210-4AB01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3593,"ΤΕΜ",1,"MC",1,"1FK22104AB010SA0"]
["1FK2210-4AB01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3593,"ΤΕΜ",1,"MC",1,"1FK22104AB010SB0"]
["1FK2210-4AB01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3902,"ΤΕΜ",1,"MC",1,"1FK22104AB011MA0"]
["1FK2210-4AB01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3902,"ΤΕΜ",1,"MC",1,"1FK22104AB011MB0"]
["1FK2210-4AB01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3593,"ΤΕΜ",1,"MC",1,"1FK22104AB011SA0"]
["1FK2210-4AB01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3593,"ΤΕΜ",1,"MC",1,"1FK22104AB011SB0"]
["1FK2210-4AB10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",4269,"ΤΕΜ",1,"MC",1,"1FK22104AB100MA0"]
["1FK2210-4AB10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4269,"ΤΕΜ",1,"MC",1,"1FK22104AB100MB0"]
["1FK2210-4AB10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3960,"ΤΕΜ",1,"MC",1,"1FK22104AB100SA0"]
["1FK2210-4AB10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3960,"ΤΕΜ",1,"MC",1,"1FK22104AB100SB0"]
["1FK2210-4AB10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",4269,"ΤΕΜ",1,"MC",1,"1FK22104AB101MA0"]
["1FK2210-4AB10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4269,"ΤΕΜ",1,"MC",1,"1FK22104AB101MB0"]
["1FK2210-4AB10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3960,"ΤΕΜ",1,"MC",1,"1FK22104AB101SA0"]
["1FK2210-4AB10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3960,"ΤΕΜ",1,"MC",1,"1FK22104AB101SB0"]
["1FK2210-4AB11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",4355,"ΤΕΜ",1,"MC",1,"1FK22104AB110MA0"]
["1FK2210-4AB11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4355,"ΤΕΜ",1,"MC",1,"1FK22104AB110MB0"]
["1FK2210-4AB11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",4046,"ΤΕΜ",1,"MC",1,"1FK22104AB110SA0"]
["1FK2210-4AB11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4046,"ΤΕΜ",1,"MC",1,"1FK22104AB110SB0"]
["1FK2210-4AB11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",4355,"ΤΕΜ",1,"MC",1,"1FK22104AB111MA0"]
["1FK2210-4AB11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4355,"ΤΕΜ",1,"MC",1,"1FK22104AB111MB0"]
["1FK2210-4AB11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",4046,"ΤΕΜ",1,"MC",1,"1FK22104AB111SA0"]
["1FK2210-4AB11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4046,"ΤΕΜ",1,"MC",1,"1FK22104AB111SB0"]
["1FK2210-4AC00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3815,"ΤΕΜ",1,"MC",1,"1FK22104AC000MA0"]
["1FK2210-4AC00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3815,"ΤΕΜ",1,"MC",1,"1FK22104AC000MB0"]
["1FK2210-4AC00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3507,"ΤΕΜ",1,"MC",1,"1FK22104AC000SA0"]
["1FK2210-4AC00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3507,"ΤΕΜ",1,"MC",1,"1FK22104AC000SB0"]
["1FK2210-4AC00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3815,"ΤΕΜ",1,"MC",1,"1FK22104AC001MA0"]
["1FK2210-4AC00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3815,"ΤΕΜ",1,"MC",1,"1FK22104AC001MB0"]
["1FK2210-4AC00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3507,"ΤΕΜ",1,"MC",1,"1FK22104AC001SA0"]
["1FK2210-4AC00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3507,"ΤΕΜ",1,"MC",1,"1FK22104AC001SB0"]
["1FK2210-4AC01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3902,"ΤΕΜ",1,"MC",1,"1FK22104AC010MA0"]
["1FK2210-4AC01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3902,"ΤΕΜ",1,"MC",1,"1FK22104AC010MB0"]
["1FK2210-4AC01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3593,"ΤΕΜ",1,"MC",1,"1FK22104AC010SA0"]
["1FK2210-4AC01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3593,"ΤΕΜ",1,"MC",1,"1FK22104AC010SB0"]
["1FK2210-4AC01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3902,"ΤΕΜ",1,"MC",1,"1FK22104AC011MA0"]
["1FK2210-4AC01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3902,"ΤΕΜ",1,"MC",1,"1FK22104AC011MB0"]
["1FK2210-4AC01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3593,"ΤΕΜ",1,"MC",1,"1FK22104AC011SA0"]
["1FK2210-4AC01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3593,"ΤΕΜ",1,"MC",1,"1FK22104AC011SB0"]
["1FK2210-4AC10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",4269,"ΤΕΜ",1,"MC",1,"1FK22104AC100MA0"]
["1FK2210-4AC10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4269,"ΤΕΜ",1,"MC",1,"1FK22104AC100MB0"]
["1FK2210-4AC10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3960,"ΤΕΜ",1,"MC",1,"1FK22104AC100SA0"]
["1FK2210-4AC10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3960,"ΤΕΜ",1,"MC",1,"1FK22104AC100SB0"]
["1FK2210-4AC10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",4269,"ΤΕΜ",1,"MC",1,"1FK22104AC101MA0"]
["1FK2210-4AC10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4269,"ΤΕΜ",1,"MC",1,"1FK22104AC101MB0"]
["1FK2210-4AC10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3960,"ΤΕΜ",1,"MC",1,"1FK22104AC101SA0"]
["1FK2210-4AC10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3960,"ΤΕΜ",1,"MC",1,"1FK22104AC101SB0"]
["1FK2210-4AC11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",4355,"ΤΕΜ",1,"MC",1,"1FK22104AC110MA0"]
["1FK2210-4AC11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4355,"ΤΕΜ",1,"MC",1,"1FK22104AC110MB0"]
["1FK2210-4AC11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",4046,"ΤΕΜ",1,"MC",1,"1FK22104AC110SA0"]
["1FK2210-4AC11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4046,"ΤΕΜ",1,"MC",1,"1FK22104AC110SB0"]
["1FK2210-4AC11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",4355,"ΤΕΜ",1,"MC",1,"1FK22104AC111MA0"]
["1FK2210-4AC11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4355,"ΤΕΜ",1,"MC",1,"1FK22104AC111MB0"]
["1FK2210-4AC11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",4046,"ΤΕΜ",1,"MC",1,"1FK22104AC111SA0"]
["1FK2210-4AC11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4046,"ΤΕΜ",1,"MC",1,"1FK22104AC111SB0"]
["1FK2210-5AC00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4442,"ΤΕΜ",1,"MC",1,"1FK22105AC000MB0"]
["1FK2210-5AC00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4134,"ΤΕΜ",1,"MC",1,"1FK22105AC000SB0"]
["1FK2210-5AC00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4442,"ΤΕΜ",1,"MC",1,"1FK22105AC001MB0"]
["1FK2210-5AC00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4134,"ΤΕΜ",1,"MC",1,"1FK22105AC001SB0"]
["1FK2210-5AC01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4529,"ΤΕΜ",1,"MC",1,"1FK22105AC010MB0"]
["1FK2210-5AC01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4220,"ΤΕΜ",1,"MC",1,"1FK22105AC010SB0"]
["1FK2210-5AC01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4529,"ΤΕΜ",1,"MC",1,"1FK22105AC011MB0"]
["1FK2210-5AC01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4220,"ΤΕΜ",1,"MC",1,"1FK22105AC011SB0"]
["1FK2210-5AC10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4896,"ΤΕΜ",1,"MC",1,"1FK22105AC100MB0"]
["1FK2210-5AC10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4587,"ΤΕΜ",1,"MC",1,"1FK22105AC100SB0"]
["1FK2210-5AC10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4896,"ΤΕΜ",1,"MC",1,"1FK22105AC101MB0"]
["1FK2210-5AC10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4587,"ΤΕΜ",1,"MC",1,"1FK22105AC101SB0"]
["1FK2210-5AC11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4982,"ΤΕΜ",1,"MC",1,"1FK22105AC110MB0"]
["1FK2210-5AC11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4673,"ΤΕΜ",1,"MC",1,"1FK22105AC110SB0"]
["1FK2210-5AC11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4982,"ΤΕΜ",1,"MC",1,"1FK22105AC111MB0"]
["1FK2210-5AC11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4673,"ΤΕΜ",1,"MC",1,"1FK22105AC111SB0"]
["1FK2306-2AC00-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1643,"ΤΕΜ",1,"MC",1,"1FK23062AC000MB0"]
["1FK2306-2AC00-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1334,"ΤΕΜ",1,"MC",1,"1FK23062AC000SB0"]
["1FK2306-2AC00-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1643,"ΤΕΜ",1,"MC",1,"1FK23062AC001MB0"]
["1FK2306-2AC00-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1334,"ΤΕΜ",1,"MC",1,"1FK23062AC001SB0"]
["1FK2306-2AC01-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1729,"ΤΕΜ",1,"MC",1,"1FK23062AC010MB0"]
["1FK2306-2AC01-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1420,"ΤΕΜ",1,"MC",1,"1FK23062AC010SB0"]
["1FK2306-2AC01-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1729,"ΤΕΜ",1,"MC",1,"1FK23062AC011MB0"]
["1FK2306-2AC01-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1420,"ΤΕΜ",1,"MC",1,"1FK23062AC011SB0"]
["1FK2306-2AC10-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1973,"ΤΕΜ",1,"MC",1,"1FK23062AC100MB0"]
["1FK2306-2AC10-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1664,"ΤΕΜ",1,"MC",1,"1FK23062AC100SB0"]
["1FK2306-2AC10-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1973,"ΤΕΜ",1,"MC",1,"1FK23062AC101MB0"]
["1FK2306-2AC10-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1664,"ΤΕΜ",1,"MC",1,"1FK23062AC101SB0"]
["1FK2306-2AC11-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2059,"ΤΕΜ",1,"MC",1,"1FK23062AC110MB0"]
["1FK2306-2AC11-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1750,"ΤΕΜ",1,"MC",1,"1FK23062AC110SB0"]
["1FK2306-2AC11-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2059,"ΤΕΜ",1,"MC",1,"1FK23062AC111MB0"]
["1FK2306-2AC11-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1750,"ΤΕΜ",1,"MC",1,"1FK23062AC111SB0"]
["1FK2306-4AC00-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2094,"ΤΕΜ",1,"MC",1,"1FK23064AC000MB0"]
["1FK2306-4AC00-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1785,"ΤΕΜ",1,"MC",1,"1FK23064AC000SB0"]
["1FK2306-4AC00-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2094,"ΤΕΜ",1,"MC",1,"1FK23064AC001MB0"]
["1FK2306-4AC00-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1785,"ΤΕΜ",1,"MC",1,"1FK23064AC001SB0"]
["1FK2306-4AC01-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2180,"ΤΕΜ",1,"MC",1,"1FK23064AC010MB0"]
["1FK2306-4AC01-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1871,"ΤΕΜ",1,"MC",1,"1FK23064AC010SB0"]
["1FK2306-4AC01-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2180,"ΤΕΜ",1,"MC",1,"1FK23064AC011MB0"]
["1FK2306-4AC01-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1871,"ΤΕΜ",1,"MC",1,"1FK23064AC011SB0"]
["1FK2306-4AC10-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2424,"ΤΕΜ",1,"MC",1,"1FK23064AC100MB0"]
["1FK2306-4AC10-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2115,"ΤΕΜ",1,"MC",1,"1FK23064AC100SB0"]
["1FK2306-4AC10-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2424,"ΤΕΜ",1,"MC",1,"1FK23064AC101MB0"]
["1FK2306-4AC10-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2115,"ΤΕΜ",1,"MC",1,"1FK23064AC101SB0"]
["1FK2306-4AC11-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2510,"ΤΕΜ",1,"MC",1,"1FK23064AC110MB0"]
["1FK2306-4AC11-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2201,"ΤΕΜ",1,"MC",1,"1FK23064AC110SB0"]
["1FK2306-4AC11-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2510,"ΤΕΜ",1,"MC",1,"1FK23064AC111MB0"]
["1FK2306-4AC11-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2201,"ΤΕΜ",1,"MC",1,"1FK23064AC111SB0"]
["1FK2308-3AB00-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2454,"ΤΕΜ",1,"MC",1,"1FK23083AB000MB0"]
["1FK2308-3AB00-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2146,"ΤΕΜ",1,"MC",1,"1FK23083AB000SB0"]
["1FK2308-3AB00-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2454,"ΤΕΜ",1,"MC",1,"1FK23083AB001MB0"]
["1FK2308-3AB00-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2146,"ΤΕΜ",1,"MC",1,"1FK23083AB001SB0"]
["1FK2308-3AB01-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2540,"ΤΕΜ",1,"MC",1,"1FK23083AB010MB0"]
["1FK2308-3AB01-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2232,"ΤΕΜ",1,"MC",1,"1FK23083AB010SB0"]
["1FK2308-3AB01-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2540,"ΤΕΜ",1,"MC",1,"1FK23083AB011MB0"]
["1FK2308-3AB01-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2232,"ΤΕΜ",1,"MC",1,"1FK23083AB011SB0"]
["1FK2308-3AB10-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2867,"ΤΕΜ",1,"MC",1,"1FK23083AB100MB0"]
["1FK2308-3AB10-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2558,"ΤΕΜ",1,"MC",1,"1FK23083AB100SB0"]
["1FK2308-3AB10-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2867,"ΤΕΜ",1,"MC",1,"1FK23083AB101MB0"]
["1FK2308-3AB10-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2558,"ΤΕΜ",1,"MC",1,"1FK23083AB101SB0"]
["1FK2308-3AB11-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2953,"ΤΕΜ",1,"MC",1,"1FK23083AB110MB0"]
["1FK2308-3AB11-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2644,"ΤΕΜ",1,"MC",1,"1FK23083AB110SB0"]
["1FK2308-3AB11-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2953,"ΤΕΜ",1,"MC",1,"1FK23083AB111MB0"]
["1FK2308-3AB11-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2644,"ΤΕΜ",1,"MC",1,"1FK23083AB111SB0"]
["1FK2308-4AB00-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2700,"ΤΕΜ",1,"MC",1,"1FK23084AB000MB0"]
["1FK2308-4AB00-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2391,"ΤΕΜ",1,"MC",1,"1FK23084AB000SB0"]
["1FK2308-4AB00-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2700,"ΤΕΜ",1,"MC",1,"1FK23084AB001MB0"]
["1FK2308-4AB00-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2391,"ΤΕΜ",1,"MC",1,"1FK23084AB001SB0"]
["1FK2308-4AB01-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2786,"ΤΕΜ",1,"MC",1,"1FK23084AB010MB0"]
["1FK2308-4AB01-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2477,"ΤΕΜ",1,"MC",1,"1FK23084AB010SB0"]
["1FK2308-4AB01-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2786,"ΤΕΜ",1,"MC",1,"1FK23084AB011MB0"]
["1FK2308-4AB01-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2477,"ΤΕΜ",1,"MC",1,"1FK23084AB011SB0"]
["1FK2308-4AB10-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3112,"ΤΕΜ",1,"MC",1,"1FK23084AB100MB0"]
["1FK2308-4AB10-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2803,"ΤΕΜ",1,"MC",1,"1FK23084AB100SB0"]
["1FK2308-4AB10-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3112,"ΤΕΜ",1,"MC",1,"1FK23084AB101MB0"]
["1FK2308-4AB10-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2803,"ΤΕΜ",1,"MC",1,"1FK23084AB101SB0"]
["1FK2308-4AB11-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3198,"ΤΕΜ",1,"MC",1,"1FK23084AB110MB0"]
["1FK2308-4AB11-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2890,"ΤΕΜ",1,"MC",1,"1FK23084AB110SB0"]
["1FK2308-4AB11-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3198,"ΤΕΜ",1,"MC",1,"1FK23084AB111MB0"]
["1FK2308-4AB11-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2890,"ΤΕΜ",1,"MC",1,"1FK23084AB111SB0"]
["1FK7011-5AK24-1AA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1435,"ΤΕΜ",1,"MC",1,"1FK70115AK241AA3"]
["1FK7011-5AK24-1AB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1686,"ΤΕΜ",1,"MC",1,"1FK70115AK241AB3"]
["1FK7011-5AK24-1AG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1387,"ΤΕΜ",1,"MC",1,"1FK70115AK241AG3"]
["1FK7011-5AK24-1AH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1584,"ΤΕΜ",1,"MC",1,"1FK70115AK241AH3"]
["1FK7011-5AK24-1JA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1285,"ΤΕΜ",1,"MC",1,"1FK70115AK241JA3"]
["1FK7011-5AK24-1JB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1536,"ΤΕΜ",1,"MC",1,"1FK70115AK241JB3"]
["1FK7011-5AK24-1JG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1237,"ΤΕΜ",1,"MC",1,"1FK70115AK241JG3"]
["1FK7011-5AK24-1JH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1434,"ΤΕΜ",1,"MC",1,"1FK70115AK241JH3"]
["1FK7011-5AK24-1SA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",781,"ΤΕΜ",1,"MC",1,"1FK70115AK241SA3"]
["1FK7011-5AK24-1SB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1032,"ΤΕΜ",1,"MC",1,"1FK70115AK241SB3"]
["1FK7011-5AK24-1SG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",733,"ΤΕΜ",1,"MC",1,"1FK70115AK241SG3"]
["1FK7011-5AK24-1SH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",930,"ΤΕΜ",1,"MC",1,"1FK70115AK241SH3"]
["1FK7011-5AK24-1TA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",781,"ΤΕΜ",1,"MC",1,"1FK70115AK241TA3"]
["1FK7011-5AK24-1TB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1032,"ΤΕΜ",1,"MC",1,"1FK70115AK241TB3"]
["1FK7011-5AK24-1TG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",733,"ΤΕΜ",1,"MC",1,"1FK70115AK241TG3"]
["1FK7011-5AK24-1TH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",930,"ΤΕΜ",1,"MC",1,"1FK70115AK241TH3"]
["1FK7011-5AK74-1AA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1435,"ΤΕΜ",1,"MC",1,"1FK70115AK741AA3"]
["1FK7011-5AK74-1AB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1686,"ΤΕΜ",1,"MC",1,"1FK70115AK741AB3"]
["1FK7011-5AK74-1AG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1387,"ΤΕΜ",1,"MC",1,"1FK70115AK741AG3"]
["1FK7011-5AK74-1AH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1584,"ΤΕΜ",1,"MC",1,"1FK70115AK741AH3"]
["1FK7011-5AK74-1JA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1285,"ΤΕΜ",1,"MC",1,"1FK70115AK741JA3"]
["1FK7011-5AK74-1JB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1536,"ΤΕΜ",1,"MC",1,"1FK70115AK741JB3"]
["1FK7011-5AK74-1JG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1237,"ΤΕΜ",1,"MC",1,"1FK70115AK741JG3"]
["1FK7011-5AK74-1JH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1434,"ΤΕΜ",1,"MC",1,"1FK70115AK741JH3"]
["1FK7011-5AK74-1SA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",781,"ΤΕΜ",1,"MC",1,"1FK70115AK741SA3"]
["1FK7011-5AK74-1SB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1032,"ΤΕΜ",1,"MC",1,"1FK70115AK741SB3"]
["1FK7011-5AK74-1SG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",733,"ΤΕΜ",1,"MC",1,"1FK70115AK741SG3"]
["1FK7011-5AK74-1SH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",930,"ΤΕΜ",1,"MC",1,"1FK70115AK741SH3"]
["1FK7011-5AK74-1TA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",781,"ΤΕΜ",1,"MC",1,"1FK70115AK741TA3"]
["1FK7011-5AK74-1TB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1032,"ΤΕΜ",1,"MC",1,"1FK70115AK741TB3"]
["1FK7011-5AK74-1TG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",733,"ΤΕΜ",1,"MC",1,"1FK70115AK741TG3"]
["1FK7011-5AK74-1TH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",930,"ΤΕΜ",1,"MC",1,"1FK70115AK741TH3"]
["1FK7015-5AK24-1AA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1527,"ΤΕΜ",1,"MC",1,"1FK70155AK241AA3"]
["1FK7015-5AK24-1AB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1778,"ΤΕΜ",1,"MC",1,"1FK70155AK241AB3"]
["1FK7015-5AK24-1AG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1479,"ΤΕΜ",1,"MC",1,"1FK70155AK241AG3"]
["1FK7015-5AK24-1AH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1676,"ΤΕΜ",1,"MC",1,"1FK70155AK241AH3"]
["1FK7015-5AK24-1JA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1377,"ΤΕΜ",1,"MC",1,"1FK70155AK241JA3"]
["1FK7015-5AK24-1JB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1628,"ΤΕΜ",1,"MC",1,"1FK70155AK241JB3"]
["1FK7015-5AK24-1JG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1329,"ΤΕΜ",1,"MC",1,"1FK70155AK241JG3"]
["1FK7015-5AK24-1JH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1526,"ΤΕΜ",1,"MC",1,"1FK70155AK241JH3"]
["1FK7015-5AK24-1SA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",873,"ΤΕΜ",1,"MC",1,"1FK70155AK241SA3"]
["1FK7015-5AK24-1SB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1124,"ΤΕΜ",1,"MC",1,"1FK70155AK241SB3"]
["1FK7015-5AK24-1SG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",825,"ΤΕΜ",1,"MC",1,"1FK70155AK241SG3"]
["1FK7015-5AK24-1SH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1022,"ΤΕΜ",1,"MC",1,"1FK70155AK241SH3"]
["1FK7015-5AK24-1TA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",873,"ΤΕΜ",1,"MC",1,"1FK70155AK241TA3"]
["1FK7015-5AK24-1TB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1124,"ΤΕΜ",1,"MC",1,"1FK70155AK241TB3"]
["1FK7015-5AK24-1TG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",825,"ΤΕΜ",1,"MC",1,"1FK70155AK241TG3"]
["1FK7015-5AK24-1TH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1022,"ΤΕΜ",1,"MC",1,"1FK70155AK241TH3"]
["1FK7015-5AK74-1AA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1527,"ΤΕΜ",1,"MC",1,"1FK70155AK741AA3"]
["1FK7015-5AK74-1AB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1778,"ΤΕΜ",1,"MC",1,"1FK70155AK741AB3"]
["1FK7015-5AK74-1AG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1479,"ΤΕΜ",1,"MC",1,"1FK70155AK741AG3"]
["1FK7015-5AK74-1AH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1676,"ΤΕΜ",1,"MC",1,"1FK70155AK741AH3"]
["1FK7015-5AK74-1JA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1377,"ΤΕΜ",1,"MC",1,"1FK70155AK741JA3"]
["1FK7015-5AK74-1JB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1628,"ΤΕΜ",1,"MC",1,"1FK70155AK741JB3"]
["1FK7015-5AK74-1JG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1329,"ΤΕΜ",1,"MC",1,"1FK70155AK741JG3"]
["1FK7015-5AK74-1JH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1526,"ΤΕΜ",1,"MC",1,"1FK70155AK741JH3"]
["1FK7015-5AK74-1SA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",873,"ΤΕΜ",1,"MC",1,"1FK70155AK741SA3"]
["1FK7015-5AK74-1SB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1124,"ΤΕΜ",1,"MC",1,"1FK70155AK741SB3"]
["1FK7015-5AK74-1SG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",825,"ΤΕΜ",1,"MC",1,"1FK70155AK741SG3"]
["1FK7015-5AK74-1SH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1022,"ΤΕΜ",1,"MC",1,"1FK70155AK741SH3"]
["1FK7015-5AK74-1TA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",873,"ΤΕΜ",1,"MC",1,"1FK70155AK741TA3"]
["1FK7015-5AK74-1TB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1124,"ΤΕΜ",1,"MC",1,"1FK70155AK741TB3"]
["1FK7015-5AK74-1TG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",825,"ΤΕΜ",1,"MC",1,"1FK70155AK741TG3"]
["1FK7015-5AK74-1TH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1022,"ΤΕΜ",1,"MC",1,"1FK70155AK741TH3"]
["1FK7022-5AF04-1AB0","SIMOTICS S-1FK7 Synchronous servo motor 1FK7 Compact; naturally cooled; NN=3000rpm; UDC=24V; IMB 5 design; Power connector rotatable; Incremental encoder sin/cos 1VSS 2048 S/R (encoder I-2048); Shaft with feather key Tolerance N with holding brake; Degree of protection IP64; Customer-specific version customer-specific motor",2006,"ΤΕΜ",1,"MC",1,"1FK70225AF041AB0"]
["1FK7022-5AK21-1DA0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2057,"ΤΕΜ",1,"MC",1,"1FK70225AK211DA0"]
["1FK7022-5AK21-1DA2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2164,"ΤΕΜ",1,"MC",1,"1FK70225AK211DA2"]
["1FK7022-5AK21-1DA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2109,"ΤΕΜ",1,"MC",1,"1FK70225AK211DA3"]
["1FK7022-5AK21-1DA5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2216,"ΤΕΜ",1,"MC",1,"1FK70225AK211DA5"]
["1FK7022-5AK21-1DA8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2331,"ΤΕΜ",1,"MC",1,"1FK70225AK211DA8"]
["1FK7022-5AK21-1DB0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2308,"ΤΕΜ",1,"MC",1,"1FK70225AK211DB0"]
["1FK7022-5AK21-1DB2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2416,"ΤΕΜ",1,"MC",1,"1FK70225AK211DB2"]
["1FK7022-5AK21-1DB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2360,"ΤΕΜ",1,"MC",1,"1FK70225AK211DB3"]
["1FK7022-5AK21-1DB5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2468,"ΤΕΜ",1,"MC",1,"1FK70225AK211DB5"]
["1FK7022-5AK21-1DB8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2582,"ΤΕΜ",1,"MC",1,"1FK70225AK211DB8"]
["1FK7022-5AK21-1DG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1958,"ΤΕΜ",1,"MC",1,"1FK70225AK211DG0"]
["1FK7022-5AK21-1DG2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2065,"ΤΕΜ",1,"MC",1,"1FK70225AK211DG2"]
["1FK7022-5AK21-1DG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2010,"ΤΕΜ",1,"MC",1,"1FK70225AK211DG3"]
["1FK7022-5AK21-1DG5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2117,"ΤΕΜ",1,"MC",1,"1FK70225AK211DG5"]
["1FK7022-5AK21-1DG8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2232,"ΤΕΜ",1,"MC",1,"1FK70225AK211DG8"]
["1FK7022-5AK21-1DH0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2206,"ΤΕΜ",1,"MC",1,"1FK70225AK211DH0"]
["1FK7022-5AK21-1DH2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2314,"ΤΕΜ",1,"MC",1,"1FK70225AK211DH2"]
["1FK7022-5AK21-1DH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2259,"ΤΕΜ",1,"MC",1,"1FK70225AK211DH3"]
["1FK7022-5AK21-1DH5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2366,"ΤΕΜ",1,"MC",1,"1FK70225AK211DH5"]
["1FK7022-5AK21-1DH8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2481,"ΤΕΜ",1,"MC",1,"1FK70225AK211DH8"]
["1FK7022-5AK21-1LA0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2481,"ΤΕΜ",1,"MC",1,"1FK70225AK211LA0"]
["1FK7022-5AK21-1LA2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2588,"ΤΕΜ",1,"MC",1,"1FK70225AK211LA2"]
["1FK7022-5AK21-1LA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2533,"ΤΕΜ",1,"MC",1,"1FK70225AK211LA3"]
["1FK7022-5AK21-1LA5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2640,"ΤΕΜ",1,"MC",1,"1FK70225AK211LA5"]
["1FK7022-5AK21-1LA8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2755,"ΤΕΜ",1,"MC",1,"1FK70225AK211LA8"]
["1FK7022-5AK21-1LB0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2732,"ΤΕΜ",1,"MC",1,"1FK70225AK211LB0"]
["1FK7022-5AK21-1LB2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2839,"ΤΕΜ",1,"MC",1,"1FK70225AK211LB2"]
["1FK7022-5AK21-1LB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2784,"ΤΕΜ",1,"MC",1,"1FK70225AK211LB3"]
["1FK7022-5AK21-1LB5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2891,"ΤΕΜ",1,"MC",1,"1FK70225AK211LB5"]
["1FK7022-5AK21-1LB8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3006,"ΤΕΜ",1,"MC",1,"1FK70225AK211LB8"]
["1FK7022-5AK21-1LG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2382,"ΤΕΜ",1,"MC",1,"1FK70225AK211LG0"]
["1FK7022-5AK21-1LG2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2489,"ΤΕΜ",1,"MC",1,"1FK70225AK211LG2"]
["1FK7022-5AK21-1LG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2434,"ΤΕΜ",1,"MC",1,"1FK70225AK211LG3"]
["1FK7022-5AK21-1LG5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2541,"ΤΕΜ",1,"MC",1,"1FK70225AK211LG5"]
["1FK7022-5AK21-1LG8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2656,"ΤΕΜ",1,"MC",1,"1FK70225AK211LG8"]
["1FK7022-5AK21-1LH0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2630,"ΤΕΜ",1,"MC",1,"1FK70225AK211LH0"]
["1FK7022-5AK21-1LH2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2738,"ΤΕΜ",1,"MC",1,"1FK70225AK211LH2"]
["1FK7022-5AK21-1LH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2682,"ΤΕΜ",1,"MC",1,"1FK70225AK211LH3"]
["1FK7022-5AK21-1LH5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2790,"ΤΕΜ",1,"MC",1,"1FK70225AK211LH5"]
["1FK7022-5AK21-1LH8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2904,"ΤΕΜ",1,"MC",1,"1FK70225AK211LH8"]
["1FK7022-5AK21-1PA0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1385,"ΤΕΜ",1,"MC",1,"1FK70225AK211PA0"]
["1FK7022-5AK21-1PA2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1492,"ΤΕΜ",1,"MC",1,"1FK70225AK211PA2"]
["1FK7022-5AK21-1PA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1437,"ΤΕΜ",1,"MC",1,"1FK70225AK211PA3"]
["1FK7022-5AK21-1PA5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1544,"ΤΕΜ",1,"MC",1,"1FK70225AK211PA5"]
["1FK7022-5AK21-1PA8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1659,"ΤΕΜ",1,"MC",1,"1FK70225AK211PA8"]
["1FK7022-5AK21-1PB0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1636,"ΤΕΜ",1,"MC",1,"1FK70225AK211PB0"]
["1FK7022-5AK21-1PB2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1743,"ΤΕΜ",1,"MC",1,"1FK70225AK211PB2"]
["1FK7022-5AK21-1PB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1688,"ΤΕΜ",1,"MC",1,"1FK70225AK211PB3"]
["1FK7022-5AK21-1PB5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1795,"ΤΕΜ",1,"MC",1,"1FK70225AK211PB5"]
["1FK7022-5AK21-1PB8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1910,"ΤΕΜ",1,"MC",1,"1FK70225AK211PB8"]
["1FK7022-5AK21-1PG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1286,"ΤΕΜ",1,"MC",1,"1FK70225AK211PG0"]
["1FK7022-5AK21-1PG2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1393,"ΤΕΜ",1,"MC",1,"1FK70225AK211PG2"]
["1FK7022-5AK21-1PG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1338,"ΤΕΜ",1,"MC",1,"1FK70225AK211PG3"]
["1FK7022-5AK21-1PG5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1445,"ΤΕΜ",1,"MC",1,"1FK70225AK211PG5"]
["1FK7022-5AK21-1PG8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1560,"ΤΕΜ",1,"MC",1,"1FK70225AK211PG8"]
["1FK7022-5AK21-1PH0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1534,"ΤΕΜ",1,"MC",1,"1FK70225AK211PH0"]
["1FK7022-5AK21-1PH2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1641,"ΤΕΜ",1,"MC",1,"1FK70225AK211PH2"]
["1FK7022-5AK21-1PH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1586,"ΤΕΜ",1,"MC",1,"1FK70225AK211PH3"]
["1FK7022-5AK21-1PH5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1693,"ΤΕΜ",1,"MC",1,"1FK70225AK211PH5"]
["1FK7022-5AK21-1PH8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1808,"ΤΕΜ",1,"MC",1,"1FK70225AK211PH8"]
["1FK7022-5AK21-1UA0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1352,"ΤΕΜ",1,"MC",1,"1FK70225AK211UA0"]
["1FK7022-5AK21-1UA2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1459,"ΤΕΜ",1,"MC",1,"1FK70225AK211UA2"]
["1FK7022-5AK21-1UA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1404,"ΤΕΜ",1,"MC",1,"1FK70225AK211UA3"]
["1FK7022-5AK21-1UA5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1511,"ΤΕΜ",1,"MC",1,"1FK70225AK211UA5"]
["1FK7022-5AK21-1UA8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1626,"ΤΕΜ",1,"MC",1,"1FK70225AK211UA8"]
["1FK7022-5AK21-1UB0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1603,"ΤΕΜ",1,"MC",1,"1FK70225AK211UB0"]
["1FK7022-5AK21-1UB2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1710,"ΤΕΜ",1,"MC",1,"1FK70225AK211UB2"]
["1FK7022-5AK21-1UB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1655,"ΤΕΜ",1,"MC",1,"1FK70225AK211UB3"]
["1FK7022-5AK21-1UB5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1762,"ΤΕΜ",1,"MC",1,"1FK70225AK211UB5"]
["1FK7022-5AK21-1UB8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1877,"ΤΕΜ",1,"MC",1,"1FK70225AK211UB8"]
["1FK7022-5AK21-1UG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1253,"ΤΕΜ",1,"MC",1,"1FK70225AK211UG0"]
["1FK7022-5AK21-1UG2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1360,"ΤΕΜ",1,"MC",1,"1FK70225AK211UG2"]
["1FK7022-5AK21-1UG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1305,"ΤΕΜ",1,"MC",1,"1FK70225AK211UG3"]
["1FK7022-5AK21-1UG5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1412,"ΤΕΜ",1,"MC",1,"1FK70225AK211UG5"]
["1FK7022-5AK21-1UG8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1527,"ΤΕΜ",1,"MC",1,"1FK70225AK211UG8"]
["1FK7022-5AK21-1UH0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1501,"ΤΕΜ",1,"MC",1,"1FK70225AK211UH0"]
["1FK7022-5AK21-1UH2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1608,"ΤΕΜ",1,"MC",1,"1FK70225AK211UH2"]
["1FK7022-5AK21-1UH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1553,"ΤΕΜ",1,"MC",1,"1FK70225AK211UH3"]
["1FK7022-5AK21-1UH5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1660,"ΤΕΜ",1,"MC",1,"1FK70225AK211UH5"]
["1FK7022-5AK21-1UH8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1775,"ΤΕΜ",1,"MC",1,"1FK70225AK211UH8"]
["1FK7022-5AK21-1VA0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1887,"ΤΕΜ",1,"MC",1,"1FK70225AK211VA0"]
["1FK7022-5AK21-1VA2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1994,"ΤΕΜ",1,"MC",1,"1FK70225AK211VA2"]
["1FK7022-5AK21-1VA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1939,"ΤΕΜ",1,"MC",1,"1FK70225AK211VA3"]
["1FK7022-5AK21-1VA5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2046,"ΤΕΜ",1,"MC",1,"1FK70225AK211VA5"]
["1FK7022-5AK21-1VA8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2161,"ΤΕΜ",1,"MC",1,"1FK70225AK211VA8"]
["1FK7022-5AK21-1VB0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2138,"ΤΕΜ",1,"MC",1,"1FK70225AK211VB0"]
["1FK7022-5AK21-1VB2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2246,"ΤΕΜ",1,"MC",1,"1FK70225AK211VB2"]
["1FK7022-5AK21-1VB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2190,"ΤΕΜ",1,"MC",1,"1FK70225AK211VB3"]
["1FK7022-5AK21-1VB5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2298,"ΤΕΜ",1,"MC",1,"1FK70225AK211VB5"]
["1FK7022-5AK21-1VB8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2412,"ΤΕΜ",1,"MC",1,"1FK70225AK211VB8"]
["1FK7022-5AK21-1VG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1788,"ΤΕΜ",1,"MC",1,"1FK70225AK211VG0"]
["1FK7022-5AK21-1VG2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1895,"ΤΕΜ",1,"MC",1,"1FK70225AK211VG2"]
["1FK7022-5AK21-1VG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1840,"ΤΕΜ",1,"MC",1,"1FK70225AK211VG3"]
["1FK7022-5AK21-1VG5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1947,"ΤΕΜ",1,"MC",1,"1FK70225AK211VG5"]
["1FK7022-5AK21-1VG8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2062,"ΤΕΜ",1,"MC",1,"1FK70225AK211VG8"]
["1FK7022-5AK21-1VH0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2037,"ΤΕΜ",1,"MC",1,"1FK70225AK211VH0"]
["1FK7022-5AK21-1VH2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2144,"ΤΕΜ",1,"MC",1,"1FK70225AK211VH2"]
["1FK7022-5AK21-1VH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2089,"ΤΕΜ",1,"MC",1,"1FK70225AK211VH3"]
["1FK7022-5AK21-1VH5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2196,"ΤΕΜ",1,"MC",1,"1FK70225AK211VH5"]
["1FK7022-5AK21-1VH8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2311,"ΤΕΜ",1,"MC",1,"1FK70225AK211VH8"]
["1FK7022-5AK24-1AA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1814,"ΤΕΜ",1,"MC",1,"1FK70225AK241AA3"]
["1FK7022-5AK24-1AA5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1921,"ΤΕΜ",1,"MC",1,"1FK70225AK241AA5"]
["1FK7022-5AK24-1AB0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2013,"ΤΕΜ",1,"MC",1,"1FK70225AK241AB0"]
["1FK7022-5AK24-1JG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1565,"ΤΕΜ",1,"MC",1,"1FK70225AK241JG3"]
["1FK7022-5AK71-1DA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2057,"ΤΕΜ",1,"MC",1,"1FK70225AK711DA0"]
["1FK7022-5AK71-1DA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2164,"ΤΕΜ",1,"MC",1,"1FK70225AK711DA2"]
["1FK7022-5AK71-1DA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2109,"ΤΕΜ",1,"MC",1,"1FK70225AK711DA3"]
["1FK7022-5AK71-1DA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2216,"ΤΕΜ",1,"MC",1,"1FK70225AK711DA5"]
["1FK7022-5AK71-1DA8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2331,"ΤΕΜ",1,"MC",1,"1FK70225AK711DA8"]
["1FK7022-5AK71-1DB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2308,"ΤΕΜ",1,"MC",1,"1FK70225AK711DB0"]
["1FK7022-5AK71-1DB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2416,"ΤΕΜ",1,"MC",1,"1FK70225AK711DB2"]
["1FK7022-5AK71-1DB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2360,"ΤΕΜ",1,"MC",1,"1FK70225AK711DB3"]
["1FK7022-5AK71-1DB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2468,"ΤΕΜ",1,"MC",1,"1FK70225AK711DB5"]
["1FK7022-5AK71-1DB8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2582,"ΤΕΜ",1,"MC",1,"1FK70225AK711DB8"]
["1FK7022-5AK71-1DG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1958,"ΤΕΜ",1,"MC",1,"1FK70225AK711DG0"]
["1FK7022-5AK71-1DG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2065,"ΤΕΜ",1,"MC",1,"1FK70225AK711DG2"]
["1FK7022-5AK71-1DG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2010,"ΤΕΜ",1,"MC",1,"1FK70225AK711DG3"]
["1FK7022-5AK71-1DG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2117,"ΤΕΜ",1,"MC",1,"1FK70225AK711DG5"]
["1FK7022-5AK71-1DG8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2232,"ΤΕΜ",1,"MC",1,"1FK70225AK711DG8"]
["1FK7022-5AK71-1DH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2206,"ΤΕΜ",1,"MC",1,"1FK70225AK711DH0"]
["1FK7022-5AK71-1DH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2314,"ΤΕΜ",1,"MC",1,"1FK70225AK711DH2"]
["1FK7022-5AK71-1DH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2259,"ΤΕΜ",1,"MC",1,"1FK70225AK711DH3"]
["1FK7022-5AK71-1DH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2366,"ΤΕΜ",1,"MC",1,"1FK70225AK711DH5"]
["1FK7022-5AK71-1DH8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2481,"ΤΕΜ",1,"MC",1,"1FK70225AK711DH8"]
["1FK7022-5AK71-1LA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2481,"ΤΕΜ",1,"MC",1,"1FK70225AK711LA0"]
["1FK7022-5AK71-1LA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2588,"ΤΕΜ",1,"MC",1,"1FK70225AK711LA2"]
["1FK7022-5AK71-1LA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2533,"ΤΕΜ",1,"MC",1,"1FK70225AK711LA3"]
["1FK7022-5AK71-1LA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2640,"ΤΕΜ",1,"MC",1,"1FK70225AK711LA5"]
["1FK7022-5AK71-1LA8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2755,"ΤΕΜ",1,"MC",1,"1FK70225AK711LA8"]
["1FK7022-5AK71-1LB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2732,"ΤΕΜ",1,"MC",1,"1FK70225AK711LB0"]
["1FK7022-5AK71-1LB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2839,"ΤΕΜ",1,"MC",1,"1FK70225AK711LB2"]
["1FK7022-5AK71-1LB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2784,"ΤΕΜ",1,"MC",1,"1FK70225AK711LB3"]
["1FK7022-5AK71-1LB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2891,"ΤΕΜ",1,"MC",1,"1FK70225AK711LB5"]
["1FK7022-5AK71-1LB8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3006,"ΤΕΜ",1,"MC",1,"1FK70225AK711LB8"]
["1FK7022-5AK71-1LG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2382,"ΤΕΜ",1,"MC",1,"1FK70225AK711LG0"]
["1FK7022-5AK71-1LG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2489,"ΤΕΜ",1,"MC",1,"1FK70225AK711LG2"]
["1FK7022-5AK71-1LG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2434,"ΤΕΜ",1,"MC",1,"1FK70225AK711LG3"]
["1FK7022-5AK71-1LG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2541,"ΤΕΜ",1,"MC",1,"1FK70225AK711LG5"]
["1FK7022-5AK71-1LG8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2656,"ΤΕΜ",1,"MC",1,"1FK70225AK711LG8"]
["1FK7022-5AK71-1LH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2630,"ΤΕΜ",1,"MC",1,"1FK70225AK711LH0"]
["1FK7022-5AK71-1LH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2738,"ΤΕΜ",1,"MC",1,"1FK70225AK711LH2"]
["1FK7022-5AK71-1LH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2682,"ΤΕΜ",1,"MC",1,"1FK70225AK711LH3"]
["1FK7022-5AK71-1LH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2790,"ΤΕΜ",1,"MC",1,"1FK70225AK711LH5"]
["1FK7022-5AK71-1LH8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2904,"ΤΕΜ",1,"MC",1,"1FK70225AK711LH8"]
["1FK7022-5AK71-1PA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1385,"ΤΕΜ",1,"MC",1,"1FK70225AK711PA0"]
["1FK7022-5AK71-1PA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1492,"ΤΕΜ",1,"MC",1,"1FK70225AK711PA2"]
["1FK7022-5AK71-1PA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1437,"ΤΕΜ",1,"MC",1,"1FK70225AK711PA3"]
["1FK7022-5AK71-1PA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1544,"ΤΕΜ",1,"MC",1,"1FK70225AK711PA5"]
["1FK7022-5AK71-1PA8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1659,"ΤΕΜ",1,"MC",1,"1FK70225AK711PA8"]
["1FK7022-5AK71-1PB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1636,"ΤΕΜ",1,"MC",1,"1FK70225AK711PB0"]
["1FK7022-5AK71-1PB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1743,"ΤΕΜ",1,"MC",1,"1FK70225AK711PB2"]
["1FK7022-5AK71-1PB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1688,"ΤΕΜ",1,"MC",1,"1FK70225AK711PB3"]
["1FK7022-5AK71-1PB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1795,"ΤΕΜ",1,"MC",1,"1FK70225AK711PB5"]
["1FK7022-5AK71-1PB8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1910,"ΤΕΜ",1,"MC",1,"1FK70225AK711PB8"]
["1FK7022-5AK71-1PG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1286,"ΤΕΜ",1,"MC",1,"1FK70225AK711PG0"]
["1FK7022-5AK71-1PG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1393,"ΤΕΜ",1,"MC",1,"1FK70225AK711PG2"]
["1FK7022-5AK71-1PG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1338,"ΤΕΜ",1,"MC",1,"1FK70225AK711PG3"]
["1FK7022-5AK71-1PG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1445,"ΤΕΜ",1,"MC",1,"1FK70225AK711PG5"]
["1FK7022-5AK71-1PG8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1560,"ΤΕΜ",1,"MC",1,"1FK70225AK711PG8"]
["1FK7022-5AK71-1PH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1534,"ΤΕΜ",1,"MC",1,"1FK70225AK711PH0"]
["1FK7022-5AK71-1PH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1641,"ΤΕΜ",1,"MC",1,"1FK70225AK711PH2"]
["1FK7022-5AK71-1PH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1586,"ΤΕΜ",1,"MC",1,"1FK70225AK711PH3"]
["1FK7022-5AK71-1PH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1693,"ΤΕΜ",1,"MC",1,"1FK70225AK711PH5"]
["1FK7022-5AK71-1PH8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1808,"ΤΕΜ",1,"MC",1,"1FK70225AK711PH8"]
["1FK7022-5AK71-1UA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1385,"ΤΕΜ",1,"MC",1,"1FK70225AK711UA0"]
["1FK7022-5AK71-1UA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1492,"ΤΕΜ",1,"MC",1,"1FK70225AK711UA2"]
["1FK7022-5AK71-1UA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1437,"ΤΕΜ",1,"MC",1,"1FK70225AK711UA3"]
["1FK7022-5AK71-1UA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1544,"ΤΕΜ",1,"MC",1,"1FK70225AK711UA5"]
["1FK7022-5AK71-1UA8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1659,"ΤΕΜ",1,"MC",1,"1FK70225AK711UA8"]
["1FK7022-5AK71-1UB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1636,"ΤΕΜ",1,"MC",1,"1FK70225AK711UB0"]
["1FK7022-5AK71-1UB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1743,"ΤΕΜ",1,"MC",1,"1FK70225AK711UB2"]
["1FK7022-5AK71-1UB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1688,"ΤΕΜ",1,"MC",1,"1FK70225AK711UB3"]
["1FK7022-5AK71-1UB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1795,"ΤΕΜ",1,"MC",1,"1FK70225AK711UB5"]
["1FK7022-5AK71-1UB8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1910,"ΤΕΜ",1,"MC",1,"1FK70225AK711UB8"]
["1FK7022-5AK71-1UG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1286,"ΤΕΜ",1,"MC",1,"1FK70225AK711UG0"]
["1FK7022-5AK71-1UG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1393,"ΤΕΜ",1,"MC",1,"1FK70225AK711UG2"]
["1FK7022-5AK71-1UG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1338,"ΤΕΜ",1,"MC",1,"1FK70225AK711UG3"]
["1FK7022-5AK71-1UG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1445,"ΤΕΜ",1,"MC",1,"1FK70225AK711UG5"]
["1FK7022-5AK71-1UG8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1560,"ΤΕΜ",1,"MC",1,"1FK70225AK711UG8"]
["1FK7022-5AK71-1UH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1534,"ΤΕΜ",1,"MC",1,"1FK70225AK711UH0"]
["1FK7022-5AK71-1UH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1641,"ΤΕΜ",1,"MC",1,"1FK70225AK711UH2"]
["1FK7022-5AK71-1UH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1586,"ΤΕΜ",1,"MC",1,"1FK70225AK711UH3"]
["1FK7022-5AK71-1UH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1693,"ΤΕΜ",1,"MC",1,"1FK70225AK711UH5"]
["1FK7022-5AK71-1UH8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1808,"ΤΕΜ",1,"MC",1,"1FK70225AK711UH8"]
["1FK7022-5AK71-1VA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1887,"ΤΕΜ",1,"MC",1,"1FK70225AK711VA0"]
["1FK7022-5AK71-1VA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1994,"ΤΕΜ",1,"MC",1,"1FK70225AK711VA2"]
["1FK7022-5AK71-1VA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1939,"ΤΕΜ",1,"MC",1,"1FK70225AK711VA3"]
["1FK7022-5AK71-1VA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2046,"ΤΕΜ",1,"MC",1,"1FK70225AK711VA5"]
["1FK7022-5AK71-1VA8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2161,"ΤΕΜ",1,"MC",1,"1FK70225AK711VA8"]
["1FK7022-5AK71-1VB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2138,"ΤΕΜ",1,"MC",1,"1FK70225AK711VB0"]
["1FK7022-5AK71-1VB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2246,"ΤΕΜ",1,"MC",1,"1FK70225AK711VB2"]
["1FK7022-5AK71-1VB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2190,"ΤΕΜ",1,"MC",1,"1FK70225AK711VB3"]
["1FK7022-5AK71-1VB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2298,"ΤΕΜ",1,"MC",1,"1FK70225AK711VB5"]
["1FK7022-5AK71-1VB8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2412,"ΤΕΜ",1,"MC",1,"1FK70225AK711VB8"]
["1FK7022-5AK71-1VG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1788,"ΤΕΜ",1,"MC",1,"1FK70225AK711VG0"]
["1FK7022-5AK71-1VG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1895,"ΤΕΜ",1,"MC",1,"1FK70225AK711VG2"]
["1FK7022-5AK71-1VG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1840,"ΤΕΜ",1,"MC",1,"1FK70225AK711VG3"]
["1FK7022-5AK71-1VG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1947,"ΤΕΜ",1,"MC",1,"1FK70225AK711VG5"]
["1FK7022-5AK71-1VG8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2062,"ΤΕΜ",1,"MC",1,"1FK70225AK711VG8"]
["1FK7022-5AK71-1VH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2037,"ΤΕΜ",1,"MC",1,"1FK70225AK711VH0"]
["1FK7022-5AK71-1VH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2144,"ΤΕΜ",1,"MC",1,"1FK70225AK711VH2"]
["1FK7022-5AK71-1VH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2089,"ΤΕΜ",1,"MC",1,"1FK70225AK711VH3"]
["1FK7022-5AK71-1VH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2196,"ΤΕΜ",1,"MC",1,"1FK70225AK711VH5"]
["1FK7022-5AK71-1VH8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2311,"ΤΕΜ",1,"MC",1,"1FK70225AK711VH8"]
["1FK7022-5AK74-1AA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1762,"ΤΕΜ",1,"MC",1,"1FK70225AK741AA0"]
["1FK7022-5AK74-1AA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1869,"ΤΕΜ",1,"MC",1,"1FK70225AK741AA2"]
["1FK7022-5AK74-1AA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1814,"ΤΕΜ",1,"MC",1,"1FK70225AK741AA3"]
["1FK7022-5AK74-1AA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1921,"ΤΕΜ",1,"MC",1,"1FK70225AK741AA5"]
["1FK7022-5AK74-1AB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2013,"ΤΕΜ",1,"MC",1,"1FK70225AK741AB0"]
["1FK7022-5AK74-1AB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2120,"ΤΕΜ",1,"MC",1,"1FK70225AK741AB2"]
["1FK7022-5AK74-1AB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2065,"ΤΕΜ",1,"MC",1,"1FK70225AK741AB3"]
["1FK7022-5AK74-1AB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2173,"ΤΕΜ",1,"MC",1,"1FK70225AK741AB5"]
["1FK7022-5AK74-1AG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1663,"ΤΕΜ",1,"MC",1,"1FK70225AK741AG0"]
["1FK7022-5AK74-1AG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1770,"ΤΕΜ",1,"MC",1,"1FK70225AK741AG2"]
["1FK7022-5AK74-1AG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1715,"ΤΕΜ",1,"MC",1,"1FK70225AK741AG3"]
["1FK7022-5AK74-1AG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1822,"ΤΕΜ",1,"MC",1,"1FK70225AK741AG5"]
["1FK7022-5AK74-1AH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1911,"ΤΕΜ",1,"MC",1,"1FK70225AK741AH0"]
["1FK7022-5AK74-1AH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2019,"ΤΕΜ",1,"MC",1,"1FK70225AK741AH2"]
["1FK7022-5AK74-1AH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1963,"ΤΕΜ",1,"MC",1,"1FK70225AK741AH3"]
["1FK7022-5AK74-1AH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2071,"ΤΕΜ",1,"MC",1,"1FK70225AK741AH5"]
["1FK7022-5AK74-1HA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2207,"ΤΕΜ",1,"MC",1,"1FK70225AK741HA0"]
["1FK7022-5AK74-1HA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2314,"ΤΕΜ",1,"MC",1,"1FK70225AK741HA2"]
["1FK7022-5AK74-1HA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2259,"ΤΕΜ",1,"MC",1,"1FK70225AK741HA3"]
["1FK7022-5AK74-1HA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2366,"ΤΕΜ",1,"MC",1,"1FK70225AK741HA5"]
["1FK7022-5AK74-1HB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2458,"ΤΕΜ",1,"MC",1,"1FK70225AK741HB0"]
["1FK7022-5AK74-1HB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2565,"ΤΕΜ",1,"MC",1,"1FK70225AK741HB2"]
["1FK7022-5AK74-1HB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2510,"ΤΕΜ",1,"MC",1,"1FK70225AK741HB3"]
["1FK7022-5AK74-1HB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2617,"ΤΕΜ",1,"MC",1,"1FK70225AK741HB5"]
["1FK7022-5AK74-1HG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2108,"ΤΕΜ",1,"MC",1,"1FK70225AK741HG0"]
["1FK7022-5AK74-1HG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2215,"ΤΕΜ",1,"MC",1,"1FK70225AK741HG2"]
["1FK7022-5AK74-1HG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2160,"ΤΕΜ",1,"MC",1,"1FK70225AK741HG3"]
["1FK7022-5AK74-1HG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2267,"ΤΕΜ",1,"MC",1,"1FK70225AK741HG5"]
["1FK7022-5AK74-1HH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2356,"ΤΕΜ",1,"MC",1,"1FK70225AK741HH0"]
["1FK7022-5AK74-1HH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2464,"ΤΕΜ",1,"MC",1,"1FK70225AK741HH2"]
["1FK7022-5AK74-1HH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2408,"ΤΕΜ",1,"MC",1,"1FK70225AK741HH3"]
["1FK7022-5AK74-1HH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2516,"ΤΕΜ",1,"MC",1,"1FK70225AK741HH5"]
["1FK7022-5AK74-1JA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1612,"ΤΕΜ",1,"MC",1,"1FK70225AK741JA0"]
["1FK7022-5AK74-1JA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1719,"ΤΕΜ",1,"MC",1,"1FK70225AK741JA2"]
["1FK7022-5AK74-1JA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1664,"ΤΕΜ",1,"MC",1,"1FK70225AK741JA3"]
["1FK7022-5AK74-1JA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1771,"ΤΕΜ",1,"MC",1,"1FK70225AK741JA5"]
["1FK7022-5AK74-1JB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1863,"ΤΕΜ",1,"MC",1,"1FK70225AK741JB0"]
["1FK7022-5AK74-1JB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1971,"ΤΕΜ",1,"MC",1,"1FK70225AK741JB2"]
["1FK7022-5AK74-1JB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1915,"ΤΕΜ",1,"MC",1,"1FK70225AK741JB3"]
["1FK7022-5AK74-1JB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2023,"ΤΕΜ",1,"MC",1,"1FK70225AK741JB5"]
["1FK7022-5AK74-1JG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1513,"ΤΕΜ",1,"MC",1,"1FK70225AK741JG0"]
["1FK7022-5AK74-1JG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1620,"ΤΕΜ",1,"MC",1,"1FK70225AK741JG2"]
["1FK7022-5AK74-1JG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1565,"ΤΕΜ",1,"MC",1,"1FK70225AK741JG3"]
["1FK7022-5AK74-1JG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1672,"ΤΕΜ",1,"MC",1,"1FK70225AK741JG5"]
["1FK7022-5AK74-1JH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1762,"ΤΕΜ",1,"MC",1,"1FK70225AK741JH0"]
["1FK7022-5AK74-1JH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1869,"ΤΕΜ",1,"MC",1,"1FK70225AK741JH2"]
["1FK7022-5AK74-1JH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1814,"ΤΕΜ",1,"MC",1,"1FK70225AK741JH3"]
["1FK7022-5AK74-1JH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1921,"ΤΕΜ",1,"MC",1,"1FK70225AK741JH5"]
["1FK7022-5AK74-1SA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1108,"ΤΕΜ",1,"MC",1,"1FK70225AK741SA0"]
["1FK7022-5AK74-1SA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1215,"ΤΕΜ",1,"MC",1,"1FK70225AK741SA2"]
["1FK7022-5AK74-1SA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1160,"ΤΕΜ",1,"MC",1,"1FK70225AK741SA3"]
["1FK7022-5AK74-1SA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1267,"ΤΕΜ",1,"MC",1,"1FK70225AK741SA5"]
["1FK7022-5AK74-1SB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1359,"ΤΕΜ",1,"MC",1,"1FK70225AK741SB0"]
["1FK7022-5AK74-1SB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1467,"ΤΕΜ",1,"MC",1,"1FK70225AK741SB2"]
["1FK7022-5AK74-1SB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1411,"ΤΕΜ",1,"MC",1,"1FK70225AK741SB3"]
["1FK7022-5AK74-1SB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1518,"ΤΕΜ",1,"MC",1,"1FK70225AK741SB5"]
["1FK7022-5AK74-1SG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1009,"ΤΕΜ",1,"MC",1,"1FK70225AK741SG0"]
["1FK7022-5AK74-1SG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1116,"ΤΕΜ",1,"MC",1,"1FK70225AK741SG2"]
["1FK7022-5AK74-1SG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1061,"ΤΕΜ",1,"MC",1,"1FK70225AK741SG3"]
["1FK7022-5AK74-1SG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1168,"ΤΕΜ",1,"MC",1,"1FK70225AK741SG5"]
["1FK7022-5AK74-1SH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1257,"ΤΕΜ",1,"MC",1,"1FK70225AK741SH0"]
["1FK7022-5AK74-1SH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1365,"ΤΕΜ",1,"MC",1,"1FK70225AK741SH2"]
["1FK7022-5AK74-1SH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1309,"ΤΕΜ",1,"MC",1,"1FK70225AK741SH3"]
["1FK7022-5AK74-1SH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1417,"ΤΕΜ",1,"MC",1,"1FK70225AK741SH5"]
["1FK7022-5AK74-1TA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1108,"ΤΕΜ",1,"MC",1,"1FK70225AK741TA0"]
["1FK7022-5AK74-1TA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1215,"ΤΕΜ",1,"MC",1,"1FK70225AK741TA2"]
["1FK7022-5AK74-1TA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1160,"ΤΕΜ",1,"MC",1,"1FK70225AK741TA3"]
["1FK7022-5AK74-1TA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1267,"ΤΕΜ",1,"MC",1,"1FK70225AK741TA5"]
["1FK7022-5AK74-1TB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1359,"ΤΕΜ",1,"MC",1,"1FK70225AK741TB0"]
["1FK7022-5AK74-1TB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1467,"ΤΕΜ",1,"MC",1,"1FK70225AK741TB2"]
["1FK7022-5AK74-1TB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1411,"ΤΕΜ",1,"MC",1,"1FK70225AK741TB3"]
["1FK7022-5AK74-1TB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1518,"ΤΕΜ",1,"MC",1,"1FK70225AK741TB5"]
["1FK7022-5AK74-1TG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1009,"ΤΕΜ",1,"MC",1,"1FK70225AK741TG0"]
["1FK7022-5AK74-1TG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1116,"ΤΕΜ",1,"MC",1,"1FK70225AK741TG2"]
["1FK7022-5AK74-1TG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1061,"ΤΕΜ",1,"MC",1,"1FK70225AK741TG3"]
["1FK7022-5AK74-1TG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1168,"ΤΕΜ",1,"MC",1,"1FK70225AK741TG5"]
["1FK7022-5AK74-1TH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1257,"ΤΕΜ",1,"MC",1,"1FK70225AK741TH0"]
["1FK7022-5AK74-1TH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1365,"ΤΕΜ",1,"MC",1,"1FK70225AK741TH2"]
["1FK7022-5AK74-1TH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1309,"ΤΕΜ",1,"MC",1,"1FK70225AK741TH3"]
["1FK7022-5AK74-1TH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1417,"ΤΕΜ",1,"MC",1,"1FK70225AK741TH5"]
["1FK7022-5AK74-8HG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, 0.85Nm 100K, 6000rpm, 0.38kW Naturally cooled Bare cable end 0.5m Outlet directions DE with connector size 1 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2346,"ΤΕΜ",1,"MC",1,"1FK70225AK748HG0"]
["1FK7022-5AK74-8HH2","SIMOTICS S Synchronous servo motor 1FK7 Compact, 0.85Nm 100K, 6000rpm, 0.38kW Naturally cooled Bare cable end 0.5m Outlet directions DE with connector size 1 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2701,"ΤΕΜ",1,"MC",1,"1FK70225AK748HH2"]
["1FK7024-5AK71-1LB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, 1.1Nm 100K, 6000rpm, 0.50kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° absolute encoder 512 S/R (encoder A-512) with DRIVE-CLiQ interface Derating 10% due to absolute encoder Shaft with feather key tolerance N with holding brake Degree of protection IP64 paint finish RAL7016",2955,"ΤΕΜ",1,"MC",1,"1FK70245AK711LB3"]
["1FK7024-5AK71-1LG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, 1.1Nm 100K, 6000rpm, 0.50kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° absolute encoder 512 S/R (encoder A-512) with DRIVE-CLiQ interface Derating 10% due to absolute encoder Smooth shaft Tolerance N without holding brake Degree of protection IP65",2553,"ΤΕΜ",1,"MC",1,"1FK70245AK711LG0"]
["1FK7024-5AK71-1LG2","SIMOTICS S Synchronous servo motor 1FK7 Compact, 1.1Nm 100K, 6000rpm, 0.50kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° absolute encoder 512 S/R (encoder A-512) with DRIVE-CLiQ interface Derating 10% due to absolute encoder Smooth shaft Tolerance N without holding brake Degree of protection IP65 DE flange IP67",2660,"ΤΕΜ",1,"MC",1,"1FK70245AK711LG2"]
["1FK7032-2AF21-1BA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",2004,"ΤΕΜ",1,"MC",1,"1FK70322AF211BA0"]
["1FK7032-2AF21-1BA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",2106,"ΤΕΜ",1,"MC",1,"1FK70322AF211BA1"]
["1FK7032-2AF21-1BA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",2106,"ΤΕΜ",1,"MC",1,"1FK70322AF211BA2"]
["1FK7032-2AF21-1BB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",2244,"ΤΕΜ",1,"MC",1,"1FK70322AF211BB0"]
["1FK7032-2AF21-1BB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",2346,"ΤΕΜ",1,"MC",1,"1FK70322AF211BB1"]
["1FK7032-2AF21-1BB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",2346,"ΤΕΜ",1,"MC",1,"1FK70322AF211BB2"]
["1FK7032-2AF21-1BG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",1910,"ΤΕΜ",1,"MC",1,"1FK70322AF211BG0"]
["1FK7032-2AF21-1BG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",2012,"ΤΕΜ",1,"MC",1,"1FK70322AF211BG1"]
["1FK7032-2AF21-1BG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",2012,"ΤΕΜ",1,"MC",1,"1FK70322AF211BG2"]
["1FK7032-2AF21-1BH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",2147,"ΤΕΜ",1,"MC",1,"1FK70322AF211BH0"]
["1FK7032-2AF21-1BH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",2249,"ΤΕΜ",1,"MC",1,"1FK70322AF211BH1"]
["1FK7032-2AF21-1BH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65, DE flange IP67",2249,"ΤΕΜ",1,"MC",1,"1FK70322AF211BH2"]
["1FK7032-2AF21-1CA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",2408,"ΤΕΜ",1,"MC",1,"1FK70322AF211CA0"]
["1FK7032-2AF21-1CA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",2510,"ΤΕΜ",1,"MC",1,"1FK70322AF211CA1"]
["1FK7032-2AF21-1CA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",2510,"ΤΕΜ",1,"MC",1,"1FK70322AF211CA2"]
["1FK7032-2AF21-1CB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",2647,"ΤΕΜ",1,"MC",1,"1FK70322AF211CB0"]
["1FK7032-2AF21-1CB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",2749,"ΤΕΜ",1,"MC",1,"1FK70322AF211CB1"]
["1FK7032-2AF21-1CB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",2749,"ΤΕΜ",1,"MC",1,"1FK70322AF211CB2"]
["1FK7032-2AF21-1CG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",2314,"ΤΕΜ",1,"MC",1,"1FK70322AF211CG0"]
["1FK7032-2AF21-1CG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",2416,"ΤΕΜ",1,"MC",1,"1FK70322AF211CG1"]
["1FK7032-2AF21-1CG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",2416,"ΤΕΜ",1,"MC",1,"1FK70322AF211CG2"]
["1FK7032-2AF21-1CH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",2550,"ΤΕΜ",1,"MC",1,"1FK70322AF211CH0"]
["1FK7032-2AF21-1CH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",2652,"ΤΕΜ",1,"MC",1,"1FK70322AF211CH1"]
["1FK7032-2AF21-1CH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65, DE flange IP67",2652,"ΤΕΜ",1,"MC",1,"1FK70322AF211CH2"]
["1FK7032-2AF21-1DA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2092,"ΤΕΜ",1,"MC",1,"1FK70322AF211DA0"]
["1FK7032-2AF21-1DA1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2192,"ΤΕΜ",1,"MC",1,"1FK70322AF211DA1"]
["1FK7032-2AF21-1DB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2331,"ΤΕΜ",1,"MC",1,"1FK70322AF211DB0"]
["1FK7032-2AF21-1DG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1998,"ΤΕΜ",1,"MC",1,"1FK70322AF211DG0"]
["1FK7032-2AF21-1DH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2234,"ΤΕΜ",1,"MC",1,"1FK70322AF211DH0"]
["1FK7032-2AF21-1FA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2495,"ΤΕΜ",1,"MC",1,"1FK70322AF211FA0"]
["1FK7032-2AF21-1FB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2735,"ΤΕΜ",1,"MC",1,"1FK70322AF211FB0"]
["1FK7032-2AF21-1FB1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2835,"ΤΕΜ",1,"MC",1,"1FK70322AF211FB1"]
["1FK7032-2AF21-1FG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2401,"ΤΕΜ",1,"MC",1,"1FK70322AF211FG0"]
["1FK7032-2AF21-1FH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2638,"ΤΕΜ",1,"MC",1,"1FK70322AF211FH0"]
["1FK7032-2AF21-1FH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2738,"ΤΕΜ",1,"MC",1,"1FK70322AF211FH2"]
["1FK7032-2AF21-1PA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP64",1364,"ΤΕΜ",1,"MC",1,"1FK70322AF211PA0"]
["1FK7032-2AF21-1PA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP65",1466,"ΤΕΜ",1,"MC",1,"1FK70322AF211PA1"]
["1FK7032-2AF21-1PA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1466,"ΤΕΜ",1,"MC",1,"1FK70322AF211PA2"]
["1FK7032-2AF21-1PB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP64",1603,"ΤΕΜ",1,"MC",1,"1FK70322AF211PB0"]
["1FK7032-2AF21-1PB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP65",1705,"ΤΕΜ",1,"MC",1,"1FK70322AF211PB1"]
["1FK7032-2AF21-1PB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1705,"ΤΕΜ",1,"MC",1,"1FK70322AF211PB2"]
["1FK7032-2AF21-1PG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP64",1269,"ΤΕΜ",1,"MC",1,"1FK70322AF211PG0"]
["1FK7032-2AF21-1PG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP65",1372,"ΤΕΜ",1,"MC",1,"1FK70322AF211PG1"]
["1FK7032-2AF21-1PG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1372,"ΤΕΜ",1,"MC",1,"1FK70322AF211PG2"]
["1FK7032-2AF21-1PH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP64",1506,"ΤΕΜ",1,"MC",1,"1FK70322AF211PH0"]
["1FK7032-2AF21-1PH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP65",1608,"ΤΕΜ",1,"MC",1,"1FK70322AF211PH1"]
["1FK7032-2AF21-1PH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1608,"ΤΕΜ",1,"MC",1,"1FK70322AF211PH2"]
["1FK7032-2AF21-1QA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",1476,"ΤΕΜ",1,"MC",1,"1FK70322AF211QA0"]
["1FK7032-2AF21-1QA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",1579,"ΤΕΜ",1,"MC",1,"1FK70322AF211QA1"]
["1FK7032-2AF21-1QA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1579,"ΤΕΜ",1,"MC",1,"1FK70322AF211QA2"]
["1FK7032-2AF21-1QB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",1716,"ΤΕΜ",1,"MC",1,"1FK70322AF211QB0"]
["1FK7032-2AF21-1QB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",1818,"ΤΕΜ",1,"MC",1,"1FK70322AF211QB1"]
["1FK7032-2AF21-1QB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",1818,"ΤΕΜ",1,"MC",1,"1FK70322AF211QB2"]
["1FK7032-2AF21-1QG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UZK=300V M0=1.2Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 power connector rotatable absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",1382,"ΤΕΜ",1,"MC",1,"1FK70322AF211QG0"]
["1FK7032-2AF21-1QG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",1484,"ΤΕΜ",1,"MC",1,"1FK70322AF211QG1"]
["1FK7032-2AF21-1QG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",1484,"ΤΕΜ",1,"MC",1,"1FK70322AF211QG2"]
["1FK7032-2AF21-1QH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",1619,"ΤΕΜ",1,"MC",1,"1FK70322AF211QH0"]
["1FK7032-2AF21-1QH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",1721,"ΤΕΜ",1,"MC",1,"1FK70322AF211QH1"]
["1FK7032-2AF21-1QH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65, DE flange IP67",1721,"ΤΕΜ",1,"MC",1,"1FK70322AF211QH2"]
["1FK7032-2AF21-1RA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",1885,"ΤΕΜ",1,"MC",1,"1FK70322AF211RA0"]
["1FK7032-2AF21-1RA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",1987,"ΤΕΜ",1,"MC",1,"1FK70322AF211RA1"]
["1FK7032-2AF21-1RA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1987,"ΤΕΜ",1,"MC",1,"1FK70322AF211RA2"]
["1FK7032-2AF21-1RB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",2125,"ΤΕΜ",1,"MC",1,"1FK70322AF211RB0"]
["1FK7032-2AF21-1RB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",2227,"ΤΕΜ",1,"MC",1,"1FK70322AF211RB1"]
["1FK7032-2AF21-1RB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",2227,"ΤΕΜ",1,"MC",1,"1FK70322AF211RB2"]
["1FK7032-2AF21-1RG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",1791,"ΤΕΜ",1,"MC",1,"1FK70322AF211RG0"]
["1FK7032-2AF21-1RG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",1893,"ΤΕΜ",1,"MC",1,"1FK70322AF211RG1"]
["1FK7032-2AF21-1RG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",1893,"ΤΕΜ",1,"MC",1,"1FK70322AF211RG2"]
["1FK7032-2AF21-1RH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",2028,"ΤΕΜ",1,"MC",1,"1FK70322AF211RH0"]
["1FK7032-2AF21-1RH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",2130,"ΤΕΜ",1,"MC",1,"1FK70322AF211RH1"]
["1FK7032-2AF21-1RH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65, DE flange IP67",2130,"ΤΕΜ",1,"MC",1,"1FK70322AF211RH2"]
["1FK7032-2AF21-1UA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP64",1364,"ΤΕΜ",1,"MC",1,"1FK70322AF211UA0"]
["1FK7032-2AF21-1UA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP65",1466,"ΤΕΜ",1,"MC",1,"1FK70322AF211UA1"]
["1FK7032-2AF21-1UA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1466,"ΤΕΜ",1,"MC",1,"1FK70322AF211UA2"]
["1FK7032-2AF21-1UB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP64",1603,"ΤΕΜ",1,"MC",1,"1FK70322AF211UB0"]
["1FK7032-2AF21-1UB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP65",1705,"ΤΕΜ",1,"MC",1,"1FK70322AF211UB1"]
["1FK7032-2AF21-1UB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1705,"ΤΕΜ",1,"MC",1,"1FK70322AF211UB2"]
["1FK7032-2AF21-1UG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP64",1269,"ΤΕΜ",1,"MC",1,"1FK70322AF211UG0"]
["1FK7032-2AF21-1UG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP65",1372,"ΤΕΜ",1,"MC",1,"1FK70322AF211UG1"]
["1FK7032-2AF21-1UG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1372,"ΤΕΜ",1,"MC",1,"1FK70322AF211UG2"]
["1FK7032-2AF21-1UH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP64",1506,"ΤΕΜ",1,"MC",1,"1FK70322AF211UH0"]
["1FK7032-2AF21-1UH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP65",1608,"ΤΕΜ",1,"MC",1,"1FK70322AF211UH1"]
["1FK7032-2AF21-1UH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1608,"ΤΕΜ",1,"MC",1,"1FK70322AF211UH2"]
["1FK7032-2AF24-1EH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2389,"ΤΕΜ",1,"MC",1,"1FK70322AF241EH2"]
["1FK7032-2AF24-1SA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP64",1100,"ΤΕΜ",1,"MC",1,"1FK70322AF241SA0"]
["1FK7032-2AF24-1SA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP65",1202,"ΤΕΜ",1,"MC",1,"1FK70322AF241SA1"]
["1FK7032-2AF24-1SA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1202,"ΤΕΜ",1,"MC",1,"1FK70322AF241SA2"]
["1FK7032-2AF24-1SB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP64",1340,"ΤΕΜ",1,"MC",1,"1FK70322AF241SB0"]
["1FK7032-2AF24-1SB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP65",1442,"ΤΕΜ",1,"MC",1,"1FK70322AF241SB1"]
["1FK7032-2AF24-1SB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",1442,"ΤΕΜ",1,"MC",1,"1FK70322AF241SB2"]
["1FK7032-2AF24-1SG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP64",1006,"ΤΕΜ",1,"MC",1,"1FK70322AF241SG0"]
["1FK7032-2AF24-1SG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP65",1108,"ΤΕΜ",1,"MC",1,"1FK70322AF241SG1"]
["1FK7032-2AF24-1SG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP65 DE flange IP67",1108,"ΤΕΜ",1,"MC",1,"1FK70322AF241SG2"]
["1FK7032-2AF24-1SH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, type of protection IP64",1243,"ΤΕΜ",1,"MC",1,"1FK70322AF241SH0"]
["1FK7032-2AF24-1SH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, type of protection IP65",1345,"ΤΕΜ",1,"MC",1,"1FK70322AF241SH1"]
["1FK7032-2AF24-1SH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, degree of protection IP65 DE Flange IP67",1345,"ΤΕΜ",1,"MC",1,"1FK70322AF241SH2"]
["1FK7032-2AF24-1TA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP64",1100,"ΤΕΜ",1,"MC",1,"1FK70322AF241TA0"]
["1FK7032-2AF24-1TA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP65",1202,"ΤΕΜ",1,"MC",1,"1FK70322AF241TA1"]
["1FK7032-2AF24-1TA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1202,"ΤΕΜ",1,"MC",1,"1FK70322AF241TA2"]
["1FK7032-2AF24-1TB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP64",1340,"ΤΕΜ",1,"MC",1,"1FK70322AF241TB0"]
["1FK7032-2AF24-1TB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP65",1442,"ΤΕΜ",1,"MC",1,"1FK70322AF241TB1"]
["1FK7032-2AF24-1TB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",1442,"ΤΕΜ",1,"MC",1,"1FK70322AF241TB2"]
["1FK7032-2AF24-1TG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP64",1006,"ΤΕΜ",1,"MC",1,"1FK70322AF241TG0"]
["1FK7032-2AF24-1TG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP65",1108,"ΤΕΜ",1,"MC",1,"1FK70322AF241TG1"]
["1FK7032-2AF24-1TG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP65 DE flange IP67",1108,"ΤΕΜ",1,"MC",1,"1FK70322AF241TG2"]
["1FK7032-2AF24-1TH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, type of protection IP64",1243,"ΤΕΜ",1,"MC",1,"1FK70322AF241TH0"]
["1FK7032-2AF24-1TH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, type of protection IP65",1345,"ΤΕΜ",1,"MC",1,"1FK70322AF241TH1"]
["1FK7032-2AF24-1TH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, degree of protection IP65 DE Flange IP67",1345,"ΤΕΜ",1,"MC",1,"1FK70322AF241TH2"]
["1FK7032-2AK71-1BA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP64",2004,"ΤΕΜ",1,"MC",1,"1FK70322AK711BA0"]
["1FK7032-2AK71-1BA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65",2106,"ΤΕΜ",1,"MC",1,"1FK70322AK711BA1"]
["1FK7032-2AK71-1BA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",2106,"ΤΕΜ",1,"MC",1,"1FK70322AK711BA2"]
["1FK7032-2AK71-1BB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP64",2244,"ΤΕΜ",1,"MC",1,"1FK70322AK711BB0"]
["1FK7032-2AK71-1BB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65",2346,"ΤΕΜ",1,"MC",1,"1FK70322AK711BB1"]
["1FK7032-2AK71-1BB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",2346,"ΤΕΜ",1,"MC",1,"1FK70322AK711BB2"]
["1FK7032-2AK71-1BG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP64",1910,"ΤΕΜ",1,"MC",1,"1FK70322AK711BG0"]
["1FK7032-2AK71-1BG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65",2012,"ΤΕΜ",1,"MC",1,"1FK70322AK711BG1"]
["1FK7032-2AK71-1BG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",2012,"ΤΕΜ",1,"MC",1,"1FK70322AK711BG2"]
["1FK7032-2AK71-1BH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP64",2147,"ΤΕΜ",1,"MC",1,"1FK70322AK711BH0"]
["1FK7032-2AK71-1BH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65",2249,"ΤΕΜ",1,"MC",1,"1FK70322AK711BH1"]
["1FK7032-2AK71-1BH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",2249,"ΤΕΜ",1,"MC",1,"1FK70322AK711BH2"]
["1FK7032-2AK71-1CA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP64",2408,"ΤΕΜ",1,"MC",1,"1FK70322AK711CA0"]
["1FK7032-2AK71-1CA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65",2510,"ΤΕΜ",1,"MC",1,"1FK70322AK711CA1"]
["1FK7032-2AK71-1CA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",2510,"ΤΕΜ",1,"MC",1,"1FK70322AK711CA2"]
["1FK7032-2AK71-1CB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP64",2647,"ΤΕΜ",1,"MC",1,"1FK70322AK711CB0"]
["1FK7032-2AK71-1CB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65",2749,"ΤΕΜ",1,"MC",1,"1FK70322AK711CB1"]
["1FK7032-2AK71-1CB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",2749,"ΤΕΜ",1,"MC",1,"1FK70322AK711CB2"]
["1FK7032-2AK71-1CG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP64",2314,"ΤΕΜ",1,"MC",1,"1FK70322AK711CG0"]
["1FK7032-2AK71-1CG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65",2416,"ΤΕΜ",1,"MC",1,"1FK70322AK711CG1"]
["1FK7032-2AK71-1CG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",2416,"ΤΕΜ",1,"MC",1,"1FK70322AK711CG2"]
["1FK7032-2AK71-1CH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP64",2550,"ΤΕΜ",1,"MC",1,"1FK70322AK711CH0"]
["1FK7032-2AK71-1CH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65",2652,"ΤΕΜ",1,"MC",1,"1FK70322AK711CH1"]
["1FK7032-2AK71-1CH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",2652,"ΤΕΜ",1,"MC",1,"1FK70322AK711CH2"]
["1FK7032-2AK71-1DA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2092,"ΤΕΜ",1,"MC",1,"1FK70322AK711DA0"]
["1FK7032-2AK71-1DA1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2192,"ΤΕΜ",1,"MC",1,"1FK70322AK711DA1"]
["1FK7032-2AK71-1DB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2331,"ΤΕΜ",1,"MC",1,"1FK70322AK711DB0"]
["1FK7032-2AK71-1DG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1998,"ΤΕΜ",1,"MC",1,"1FK70322AK711DG0"]
["1FK7032-2AK71-1DG1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2098,"ΤΕΜ",1,"MC",1,"1FK70322AK711DG1"]
["1FK7032-2AK71-1DG2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2098,"ΤΕΜ",1,"MC",1,"1FK70322AK711DG2"]
["1FK7032-2AK71-1DH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2234,"ΤΕΜ",1,"MC",1,"1FK70322AK711DH0"]
["1FK7032-2AK71-1DH1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2334,"ΤΕΜ",1,"MC",1,"1FK70322AK711DH1"]
["1FK7032-2AK71-1FA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2495,"ΤΕΜ",1,"MC",1,"1FK70322AK711FA0"]
["1FK7032-2AK71-1FA2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2596,"ΤΕΜ",1,"MC",1,"1FK70322AK711FA2"]
["1FK7032-2AK71-1FB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2735,"ΤΕΜ",1,"MC",1,"1FK70322AK711FB0"]
["1FK7032-2AK71-1FB1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2835,"ΤΕΜ",1,"MC",1,"1FK70322AK711FB1"]
["1FK7032-2AK71-1FG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2401,"ΤΕΜ",1,"MC",1,"1FK70322AK711FG0"]
["1FK7032-2AK71-1FG1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2501,"ΤΕΜ",1,"MC",1,"1FK70322AK711FG1"]
["1FK7032-2AK71-1FH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2638,"ΤΕΜ",1,"MC",1,"1FK70322AK711FH0"]
["1FK7032-2AK71-1FH1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2738,"ΤΕΜ",1,"MC",1,"1FK70322AK711FH1"]
["1FK7032-2AK71-1PA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP64",1364,"ΤΕΜ",1,"MC",1,"1FK70322AK711PA0"]
["1FK7032-2AK71-1PA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP65",1466,"ΤΕΜ",1,"MC",1,"1FK70322AK711PA1"]
["1FK7032-2AK71-1PA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1466,"ΤΕΜ",1,"MC",1,"1FK70322AK711PA2"]
["1FK7032-2AK71-1PB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP64",1603,"ΤΕΜ",1,"MC",1,"1FK70322AK711PB0"]
["1FK7032-2AK71-1PB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP65",1705,"ΤΕΜ",1,"MC",1,"1FK70322AK711PB1"]
["1FK7032-2AK71-1PB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1705,"ΤΕΜ",1,"MC",1,"1FK70322AK711PB2"]
["1FK7032-2AK71-1PG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP64",1269,"ΤΕΜ",1,"MC",1,"1FK70322AK711PG0"]
["1FK7032-2AK71-1PG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP65",1372,"ΤΕΜ",1,"MC",1,"1FK70322AK711PG1"]
["1FK7032-2AK71-1PG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1372,"ΤΕΜ",1,"MC",1,"1FK70322AK711PG2"]
["1FK7032-2AK71-1PH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP64",1506,"ΤΕΜ",1,"MC",1,"1FK70322AK711PH0"]
["1FK7032-2AK71-1PH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP65",1608,"ΤΕΜ",1,"MC",1,"1FK70322AK711PH1"]
["1FK7032-2AK71-1PH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1608,"ΤΕΜ",1,"MC",1,"1FK70322AK711PH2"]
["1FK7032-2AK71-1QA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP64",1476,"ΤΕΜ",1,"MC",1,"1FK70322AK711QA0"]
["1FK7032-2AK71-1QA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65",1579,"ΤΕΜ",1,"MC",1,"1FK70322AK711QA1"]
["1FK7032-2AK71-1QA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",1579,"ΤΕΜ",1,"MC",1,"1FK70322AK711QA2"]
["1FK7032-2AK71-1QB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP64",1716,"ΤΕΜ",1,"MC",1,"1FK70322AK711QB0"]
["1FK7032-2AK71-1QB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65",1818,"ΤΕΜ",1,"MC",1,"1FK70322AK711QB1"]
["1FK7032-2AK71-1QB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",1818,"ΤΕΜ",1,"MC",1,"1FK70322AK711QB2"]
["1FK7032-2AK71-1QG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP64",1382,"ΤΕΜ",1,"MC",1,"1FK70322AK711QG0"]
["1FK7032-2AK71-1QG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65",1484,"ΤΕΜ",1,"MC",1,"1FK70322AK711QG1"]
["1FK7032-2AK71-1QG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",1484,"ΤΕΜ",1,"MC",1,"1FK70322AK711QG2"]
["1FK7032-2AK71-1QH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP64",1619,"ΤΕΜ",1,"MC",1,"1FK70322AK711QH0"]
["1FK7032-2AK71-1QH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65",1721,"ΤΕΜ",1,"MC",1,"1FK70322AK711QH1"]
["1FK7032-2AK71-1QH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",1721,"ΤΕΜ",1,"MC",1,"1FK70322AK711QH2"]
["1FK7032-2AK71-1RA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP64",1885,"ΤΕΜ",1,"MC",1,"1FK70322AK711RA0"]
["1FK7032-2AK71-1RA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65",1987,"ΤΕΜ",1,"MC",1,"1FK70322AK711RA1"]
["1FK7032-2AK71-1RA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",1987,"ΤΕΜ",1,"MC",1,"1FK70322AK711RA2"]
["1FK7032-2AK71-1RB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP64",2125,"ΤΕΜ",1,"MC",1,"1FK70322AK711RB0"]
["1FK7032-2AK71-1RB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65",2227,"ΤΕΜ",1,"MC",1,"1FK70322AK711RB1"]
["1FK7032-2AK71-1RB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",2227,"ΤΕΜ",1,"MC",1,"1FK70322AK711RB2"]
["1FK7032-2AK71-1RG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP64",1791,"ΤΕΜ",1,"MC",1,"1FK70322AK711RG0"]
["1FK7032-2AK71-1RG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65",1893,"ΤΕΜ",1,"MC",1,"1FK70322AK711RG1"]
["1FK7032-2AK71-1RG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",1893,"ΤΕΜ",1,"MC",1,"1FK70322AK711RG2"]
["1FK7032-2AK71-1RH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP64",2028,"ΤΕΜ",1,"MC",1,"1FK70322AK711RH0"]
["1FK7032-2AK71-1RH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65",2130,"ΤΕΜ",1,"MC",1,"1FK70322AK711RH1"]
["1FK7032-2AK71-1RH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",2130,"ΤΕΜ",1,"MC",1,"1FK70322AK711RH2"]
["1FK7032-2AK71-1UA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP64",1364,"ΤΕΜ",1,"MC",1,"1FK70322AK711UA0"]
["1FK7032-2AK71-1UA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP65",1466,"ΤΕΜ",1,"MC",1,"1FK70322AK711UA1"]
["1FK7032-2AK71-1UA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1466,"ΤΕΜ",1,"MC",1,"1FK70322AK711UA2"]
["1FK7032-2AK71-1UB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP64",1603,"ΤΕΜ",1,"MC",1,"1FK70322AK711UB0"]
["1FK7032-2AK71-1UB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP65",1705,"ΤΕΜ",1,"MC",1,"1FK70322AK711UB1"]
["1FK7032-2AK71-1UB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1705,"ΤΕΜ",1,"MC",1,"1FK70322AK711UB2"]
["1FK7032-2AK71-1UG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP64",1269,"ΤΕΜ",1,"MC",1,"1FK70322AK711UG0"]
["1FK7032-2AK71-1UG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP65",1372,"ΤΕΜ",1,"MC",1,"1FK70322AK711UG1"]
["1FK7032-2AK71-1UG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1372,"ΤΕΜ",1,"MC",1,"1FK70322AK711UG2"]
["1FK7032-2AK71-1UH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP64",1506,"ΤΕΜ",1,"MC",1,"1FK70322AK711UH0"]
["1FK7032-2AK71-1UH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP65",1608,"ΤΕΜ",1,"MC",1,"1FK70322AK711UH1"]
["1FK7032-2AK71-1UH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1608,"ΤΕΜ",1,"MC",1,"1FK70322AK711UH2"]
["1FK7032-2AK74-1AA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1741,"ΤΕΜ",1,"MC",1,"1FK70322AK741AA0"]
["1FK7032-2AK74-1AA1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1841,"ΤΕΜ",1,"MC",1,"1FK70322AK741AA1"]
["1FK7032-2AK74-1AA2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1841,"ΤΕΜ",1,"MC",1,"1FK70322AK741AA2"]
["1FK7032-2AK74-1AB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1980,"ΤΕΜ",1,"MC",1,"1FK70322AK741AB0"]
["1FK7032-2AK74-1AB1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2080,"ΤΕΜ",1,"MC",1,"1FK70322AK741AB1"]
["1FK7032-2AK74-1AB2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2080,"ΤΕΜ",1,"MC",1,"1FK70322AK741AB2"]
["1FK7032-2AK74-1AG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1646,"ΤΕΜ",1,"MC",1,"1FK70322AK741AG0"]
["1FK7032-2AK74-1AG1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1747,"ΤΕΜ",1,"MC",1,"1FK70322AK741AG1"]
["1FK7032-2AK74-1AG2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1747,"ΤΕΜ",1,"MC",1,"1FK70322AK741AG2"]
["1FK7032-2AK74-1AH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1883,"ΤΕΜ",1,"MC",1,"1FK70322AK741AH0"]
["1FK7032-2AK74-1AH1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1983,"ΤΕΜ",1,"MC",1,"1FK70322AK741AH1"]
["1FK7032-2AK74-1AH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1983,"ΤΕΜ",1,"MC",1,"1FK70322AK741AH2"]
["1FK7032-2AK74-1EA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2147,"ΤΕΜ",1,"MC",1,"1FK70322AK741EA0"]
["1FK7032-2AK74-1EA1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2247,"ΤΕΜ",1,"MC",1,"1FK70322AK741EA1"]
["1FK7032-2AK74-1EA2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2247,"ΤΕΜ",1,"MC",1,"1FK70322AK741EA2"]
["1FK7032-2AK74-1EB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2386,"ΤΕΜ",1,"MC",1,"1FK70322AK741EB0"]
["1FK7032-2AK74-1EB1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2486,"ΤΕΜ",1,"MC",1,"1FK70322AK741EB1"]
["1FK7032-2AK74-1EB2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2486,"ΤΕΜ",1,"MC",1,"1FK70322AK741EB2"]
["1FK7032-2AK74-1EG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2053,"ΤΕΜ",1,"MC",1,"1FK70322AK741EG0"]
["1FK7032-2AK74-1EG1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2153,"ΤΕΜ",1,"MC",1,"1FK70322AK741EG1"]
["1FK7032-2AK74-1EG2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2153,"ΤΕΜ",1,"MC",1,"1FK70322AK741EG2"]
["1FK7032-2AK74-1EH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2289,"ΤΕΜ",1,"MC",1,"1FK70322AK741EH0"]
["1FK7032-2AK74-1EH1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2389,"ΤΕΜ",1,"MC",1,"1FK70322AK741EH1"]
["1FK7032-2AK74-1EH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2389,"ΤΕΜ",1,"MC",1,"1FK70322AK741EH2"]
["1FK7032-2AK74-1SA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP64",1100,"ΤΕΜ",1,"MC",1,"1FK70322AK741SA0"]
["1FK7032-2AK74-1SA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP65",1202,"ΤΕΜ",1,"MC",1,"1FK70322AK741SA1"]
["1FK7032-2AK74-1SA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1202,"ΤΕΜ",1,"MC",1,"1FK70322AK741SA2"]
["1FK7032-2AK74-1SB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP64",1340,"ΤΕΜ",1,"MC",1,"1FK70322AK741SB0"]
["1FK7032-2AK74-1SB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP65",1442,"ΤΕΜ",1,"MC",1,"1FK70322AK741SB1"]
["1FK7032-2AK74-1SB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",1442,"ΤΕΜ",1,"MC",1,"1FK70322AK741SB2"]
["1FK7032-2AK74-1SG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP64",1006,"ΤΕΜ",1,"MC",1,"1FK70322AK741SG0"]
["1FK7032-2AK74-1SG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP65",1108,"ΤΕΜ",1,"MC",1,"1FK70322AK741SG1"]
["1FK7032-2AK74-1SG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP65 DE flange IP67",1108,"ΤΕΜ",1,"MC",1,"1FK70322AK741SG2"]
["1FK7032-2AK74-1SH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, type of protection IP64",1243,"ΤΕΜ",1,"MC",1,"1FK70322AK741SH0"]
["1FK7032-2AK74-1SH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, type of protection IP65",1345,"ΤΕΜ",1,"MC",1,"1FK70322AK741SH1"]
["1FK7032-2AK74-1SH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1345,"ΤΕΜ",1,"MC",1,"1FK70322AK741SH2"]
["1FK7032-2AK74-1TA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP64",1100,"ΤΕΜ",1,"MC",1,"1FK70322AK741TA0"]
["1FK7032-2AK74-1TA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP65",1202,"ΤΕΜ",1,"MC",1,"1FK70322AK741TA1"]
["1FK7032-2AK74-1TA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1202,"ΤΕΜ",1,"MC",1,"1FK70322AK741TA2"]
["1FK7032-2AK74-1TB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP64",1340,"ΤΕΜ",1,"MC",1,"1FK70322AK741TB0"]
["1FK7032-2AK74-1TB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP65",1442,"ΤΕΜ",1,"MC",1,"1FK70322AK741TB1"]
["1FK7032-2AK74-1TB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",1442,"ΤΕΜ",1,"MC",1,"1FK70322AK741TB2"]
["1FK7032-2AK74-1TG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP64",1006,"ΤΕΜ",1,"MC",1,"1FK70322AK741TG0"]
["1FK7032-2AK74-1TG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP65",1108,"ΤΕΜ",1,"MC",1,"1FK70322AK741TG1"]
["1FK7032-2AK74-1TG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP65 DE flange IP67",1108,"ΤΕΜ",1,"MC",1,"1FK70322AK741TG2"]
["1FK7032-2AK74-1TH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, type of protection IP64",1243,"ΤΕΜ",1,"MC",1,"1FK70322AK741TH0"]
["1FK7032-2AK74-1TH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, type of protection IP65",1345,"ΤΕΜ",1,"MC",1,"1FK70322AK741TH1"]
["1FK7032-2AK74-1TH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1345,"ΤΕΜ",1,"MC",1,"1FK70322AK741TH2"]
["1FK7033-4CF21-1BA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2053,"ΤΕΜ",1,"MC",1,"1FK70334CF211BA0"]
["1FK7033-4CF21-1BA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2153,"ΤΕΜ",1,"MC",1,"1FK70334CF211BA1"]
["1FK7033-4CF21-1BA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2153,"ΤΕΜ",1,"MC",1,"1FK70334CF211BA2"]
["1FK7033-4CF21-1BB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2292,"ΤΕΜ",1,"MC",1,"1FK70334CF211BB0"]
["1FK7033-4CF21-1BB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2392,"ΤΕΜ",1,"MC",1,"1FK70334CF211BB1"]
["1FK7033-4CF21-1BB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2392,"ΤΕΜ",1,"MC",1,"1FK70334CF211BB2"]
["1FK7033-4CF21-1BG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1958,"ΤΕΜ",1,"MC",1,"1FK70334CF211BG0"]
["1FK7033-4CF21-1BG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2059,"ΤΕΜ",1,"MC",1,"1FK70334CF211BG1"]
["1FK7033-4CF21-1BG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2059,"ΤΕΜ",1,"MC",1,"1FK70334CF211BG2"]
["1FK7033-4CF21-1BH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2195,"ΤΕΜ",1,"MC",1,"1FK70334CF211BH0"]
["1FK7033-4CF21-1BH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2295,"ΤΕΜ",1,"MC",1,"1FK70334CF211BH1"]
["1FK7033-4CF21-1BH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2295,"ΤΕΜ",1,"MC",1,"1FK70334CF211BH2"]
["1FK7033-4CF21-1CA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2456,"ΤΕΜ",1,"MC",1,"1FK70334CF211CA0"]
["1FK7033-4CF21-1CA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2556,"ΤΕΜ",1,"MC",1,"1FK70334CF211CA1"]
["1FK7033-4CF21-1CA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2556,"ΤΕΜ",1,"MC",1,"1FK70334CF211CA2"]
["1FK7033-4CF21-1CB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2695,"ΤΕΜ",1,"MC",1,"1FK70334CF211CB0"]
["1FK7033-4CF21-1CB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2796,"ΤΕΜ",1,"MC",1,"1FK70334CF211CB1"]
["1FK7033-4CF21-1CB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2796,"ΤΕΜ",1,"MC",1,"1FK70334CF211CB2"]
["1FK7033-4CF21-1CG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2362,"ΤΕΜ",1,"MC",1,"1FK70334CF211CG0"]
["1FK7033-4CF21-1CG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2462,"ΤΕΜ",1,"MC",1,"1FK70334CF211CG1"]
["1FK7033-4CF21-1CG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2462,"ΤΕΜ",1,"MC",1,"1FK70334CF211CG2"]
["1FK7033-4CF21-1CH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2599,"ΤΕΜ",1,"MC",1,"1FK70334CF211CH0"]
["1FK7033-4CF21-1CH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2699,"ΤΕΜ",1,"MC",1,"1FK70334CF211CH1"]
["1FK7033-4CF21-1CH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2699,"ΤΕΜ",1,"MC",1,"1FK70334CF211CH2"]
["1FK7033-4CF21-1DA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2140,"ΤΕΜ",1,"MC",1,"1FK70334CF211DA0"]
["1FK7033-4CF21-1DA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2240,"ΤΕΜ",1,"MC",1,"1FK70334CF211DA1"]
["1FK7033-4CF21-1DH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2383,"ΤΕΜ",1,"MC",1,"1FK70334CF211DH1"]
["1FK7033-4CF21-1PA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1412,"ΤΕΜ",1,"MC",1,"1FK70334CF211PA0"]
["1FK7033-4CF21-1PA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1512,"ΤΕΜ",1,"MC",1,"1FK70334CF211PA1"]
["1FK7033-4CF21-1PA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1512,"ΤΕΜ",1,"MC",1,"1FK70334CF211PA2"]
["1FK7033-4CF21-1PB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1651,"ΤΕΜ",1,"MC",1,"1FK70334CF211PB0"]
["1FK7033-4CF21-1PB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1752,"ΤΕΜ",1,"MC",1,"1FK70334CF211PB1"]
["1FK7033-4CF21-1PB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1752,"ΤΕΜ",1,"MC",1,"1FK70334CF211PB2"]
["1FK7033-4CF21-1PG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1318,"ΤΕΜ",1,"MC",1,"1FK70334CF211PG0"]
["1FK7033-4CF21-1PG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1418,"ΤΕΜ",1,"MC",1,"1FK70334CF211PG1"]
["1FK7033-4CF21-1PG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1418,"ΤΕΜ",1,"MC",1,"1FK70334CF211PG2"]
["1FK7033-4CF21-1PH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1554,"ΤΕΜ",1,"MC",1,"1FK70334CF211PH0"]
["1FK7033-4CF21-1PH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1655,"ΤΕΜ",1,"MC",1,"1FK70334CF211PH1"]
["1FK7033-4CF21-1PH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1655,"ΤΕΜ",1,"MC",1,"1FK70334CF211PH2"]
["1FK7033-4CF21-1QA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1525,"ΤΕΜ",1,"MC",1,"1FK70334CF211QA0"]
["1FK7033-4CF21-1QA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1625,"ΤΕΜ",1,"MC",1,"1FK70334CF211QA1"]
["1FK7033-4CF21-1QA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1625,"ΤΕΜ",1,"MC",1,"1FK70334CF211QA2"]
["1FK7033-4CF21-1QB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1764,"ΤΕΜ",1,"MC",1,"1FK70334CF211QB0"]
["1FK7033-4CF21-1QB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1864,"ΤΕΜ",1,"MC",1,"1FK70334CF211QB1"]
["1FK7033-4CF21-1QB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1864,"ΤΕΜ",1,"MC",1,"1FK70334CF211QB2"]
["1FK7033-4CF21-1QG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1430,"ΤΕΜ",1,"MC",1,"1FK70334CF211QG0"]
["1FK7033-4CF21-1QG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1531,"ΤΕΜ",1,"MC",1,"1FK70334CF211QG1"]
["1FK7033-4CF21-1QG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1531,"ΤΕΜ",1,"MC",1,"1FK70334CF211QG2"]
["1FK7033-4CF21-1QH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1667,"ΤΕΜ",1,"MC",1,"1FK70334CF211QH0"]
["1FK7033-4CF21-1QH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1767,"ΤΕΜ",1,"MC",1,"1FK70334CF211QH1"]
["1FK7033-4CF21-1QH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1767,"ΤΕΜ",1,"MC",1,"1FK70334CF211QH2"]
["1FK7033-4CF21-1RA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1934,"ΤΕΜ",1,"MC",1,"1FK70334CF211RA0"]
["1FK7033-4CF21-1RA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2034,"ΤΕΜ",1,"MC",1,"1FK70334CF211RA1"]
["1FK7033-4CF21-1RA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2034,"ΤΕΜ",1,"MC",1,"1FK70334CF211RA2"]
["1FK7033-4CF21-1RB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2173,"ΤΕΜ",1,"MC",1,"1FK70334CF211RB0"]
["1FK7033-4CF21-1RB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2273,"ΤΕΜ",1,"MC",1,"1FK70334CF211RB1"]
["1FK7033-4CF21-1RB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2273,"ΤΕΜ",1,"MC",1,"1FK70334CF211RB2"]
["1FK7033-4CF21-1RG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1839,"ΤΕΜ",1,"MC",1,"1FK70334CF211RG0"]
["1FK7033-4CF21-1RG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1940,"ΤΕΜ",1,"MC",1,"1FK70334CF211RG1"]
["1FK7033-4CF21-1RG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1940,"ΤΕΜ",1,"MC",1,"1FK70334CF211RG2"]
["1FK7033-4CF21-1RH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2076,"ΤΕΜ",1,"MC",1,"1FK70334CF211RH0"]
["1FK7033-4CF21-1RH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2176,"ΤΕΜ",1,"MC",1,"1FK70334CF211RH1"]
["1FK7033-4CF21-1RH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2176,"ΤΕΜ",1,"MC",1,"1FK70334CF211RH2"]
["1FK7033-4CF21-1UA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1412,"ΤΕΜ",1,"MC",1,"1FK70334CF211UA0"]
["1FK7033-4CF21-1UA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1512,"ΤΕΜ",1,"MC",1,"1FK70334CF211UA1"]
["1FK7033-4CF21-1UA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1512,"ΤΕΜ",1,"MC",1,"1FK70334CF211UA2"]
["1FK7033-4CF21-1UB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1651,"ΤΕΜ",1,"MC",1,"1FK70334CF211UB0"]
["1FK7033-4CF21-1UB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1752,"ΤΕΜ",1,"MC",1,"1FK70334CF211UB1"]
["1FK7033-4CF21-1UB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1752,"ΤΕΜ",1,"MC",1,"1FK70334CF211UB2"]
["1FK7033-4CF21-1UG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1318,"ΤΕΜ",1,"MC",1,"1FK70334CF211UG0"]
["1FK7033-4CF21-1UG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1418,"ΤΕΜ",1,"MC",1,"1FK70334CF211UG1"]
["1FK7033-4CF21-1UG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1418,"ΤΕΜ",1,"MC",1,"1FK70334CF211UG2"]
["1FK7033-4CF21-1UH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1554,"ΤΕΜ",1,"MC",1,"1FK70334CF211UH0"]
["1FK7033-4CF21-1UH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1655,"ΤΕΜ",1,"MC",1,"1FK70334CF211UH1"]
["1FK7033-4CF21-1UH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1655,"ΤΕΜ",1,"MC",1,"1FK70334CF211UH2"]
["1FK7033-4CF24-1AH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1931,"ΤΕΜ",1,"MC",1,"1FK70334CF241AH0"]
["1FK7033-4CF24-1EG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2101,"ΤΕΜ",1,"MC",1,"1FK70334CF241EG0"]
["1FK7033-4CK71-1BA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2053,"ΤΕΜ",1,"MC",1,"1FK70334CK711BA0"]
["1FK7033-4CK71-1BA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2153,"ΤΕΜ",1,"MC",1,"1FK70334CK711BA1"]
["1FK7033-4CK71-1BA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2153,"ΤΕΜ",1,"MC",1,"1FK70334CK711BA2"]
["1FK7033-4CK71-1BB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2292,"ΤΕΜ",1,"MC",1,"1FK70334CK711BB0"]
["1FK7033-4CK71-1BB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2392,"ΤΕΜ",1,"MC",1,"1FK70334CK711BB1"]
["1FK7033-4CK71-1BB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2392,"ΤΕΜ",1,"MC",1,"1FK70334CK711BB2"]
["1FK7033-4CK71-1BG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1958,"ΤΕΜ",1,"MC",1,"1FK70334CK711BG0"]
["1FK7033-4CK71-1BG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2059,"ΤΕΜ",1,"MC",1,"1FK70334CK711BG1"]
["1FK7033-4CK71-1BG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2059,"ΤΕΜ",1,"MC",1,"1FK70334CK711BG2"]
["1FK7033-4CK71-1BH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2195,"ΤΕΜ",1,"MC",1,"1FK70334CK711BH0"]
["1FK7033-4CK71-1BH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2295,"ΤΕΜ",1,"MC",1,"1FK70334CK711BH1"]
["1FK7033-4CK71-1BH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2295,"ΤΕΜ",1,"MC",1,"1FK70334CK711BH2"]
["1FK7033-4CK71-1CA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2456,"ΤΕΜ",1,"MC",1,"1FK70334CK711CA0"]
["1FK7033-4CK71-1CA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2556,"ΤΕΜ",1,"MC",1,"1FK70334CK711CA1"]
["1FK7033-4CK71-1CA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2556,"ΤΕΜ",1,"MC",1,"1FK70334CK711CA2"]
["1FK7033-4CK71-1CB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2695,"ΤΕΜ",1,"MC",1,"1FK70334CK711CB0"]
["1FK7033-4CK71-1CB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2796,"ΤΕΜ",1,"MC",1,"1FK70334CK711CB1"]
["1FK7033-4CK71-1CB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2796,"ΤΕΜ",1,"MC",1,"1FK70334CK711CB2"]
["1FK7033-4CK71-1CG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2362,"ΤΕΜ",1,"MC",1,"1FK70334CK711CG0"]
["1FK7033-4CK71-1CG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2462,"ΤΕΜ",1,"MC",1,"1FK70334CK711CG1"]
["1FK7033-4CK71-1CG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2462,"ΤΕΜ",1,"MC",1,"1FK70334CK711CG2"]
["1FK7033-4CK71-1CH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2599,"ΤΕΜ",1,"MC",1,"1FK70334CK711CH0"]
["1FK7033-4CK71-1CH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2699,"ΤΕΜ",1,"MC",1,"1FK70334CK711CH1"]
["1FK7033-4CK71-1CH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2699,"ΤΕΜ",1,"MC",1,"1FK70334CK711CH2"]
["1FK7033-4CK71-1DA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2140,"ΤΕΜ",1,"MC",1,"1FK70334CK711DA0"]
["1FK7033-4CK71-1DA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2240,"ΤΕΜ",1,"MC",1,"1FK70334CK711DA2"]
["1FK7033-4CK71-1DG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2046,"ΤΕΜ",1,"MC",1,"1FK70334CK711DG0"]
["1FK7033-4CK71-1PA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1412,"ΤΕΜ",1,"MC",1,"1FK70334CK711PA0"]
["1FK7033-4CK71-1PA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1512,"ΤΕΜ",1,"MC",1,"1FK70334CK711PA1"]
["1FK7033-4CK71-1PA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1512,"ΤΕΜ",1,"MC",1,"1FK70334CK711PA2"]
["1FK7033-4CK71-1PB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1651,"ΤΕΜ",1,"MC",1,"1FK70334CK711PB0"]
["1FK7033-4CK71-1PB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1752,"ΤΕΜ",1,"MC",1,"1FK70334CK711PB1"]
["1FK7033-4CK71-1PB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1752,"ΤΕΜ",1,"MC",1,"1FK70334CK711PB2"]
["1FK7033-4CK71-1PG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1318,"ΤΕΜ",1,"MC",1,"1FK70334CK711PG0"]
["1FK7033-4CK71-1PG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1418,"ΤΕΜ",1,"MC",1,"1FK70334CK711PG1"]
["1FK7033-4CK71-1PG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1418,"ΤΕΜ",1,"MC",1,"1FK70334CK711PG2"]
["1FK7033-4CK71-1PH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1554,"ΤΕΜ",1,"MC",1,"1FK70334CK711PH0"]
["1FK7033-4CK71-1PH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1655,"ΤΕΜ",1,"MC",1,"1FK70334CK711PH1"]
["1FK7033-4CK71-1PH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1655,"ΤΕΜ",1,"MC",1,"1FK70334CK711PH2"]
["1FK7033-4CK71-1QA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1525,"ΤΕΜ",1,"MC",1,"1FK70334CK711QA0"]
["1FK7033-4CK71-1QA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1625,"ΤΕΜ",1,"MC",1,"1FK70334CK711QA1"]
["1FK7033-4CK71-1QA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1625,"ΤΕΜ",1,"MC",1,"1FK70334CK711QA2"]
["1FK7033-4CK71-1QB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1764,"ΤΕΜ",1,"MC",1,"1FK70334CK711QB0"]
["1FK7033-4CK71-1QB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1864,"ΤΕΜ",1,"MC",1,"1FK70334CK711QB1"]
["1FK7033-4CK71-1QB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1864,"ΤΕΜ",1,"MC",1,"1FK70334CK711QB2"]
["1FK7033-4CK71-1QG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1430,"ΤΕΜ",1,"MC",1,"1FK70334CK711QG0"]
["1FK7033-4CK71-1QG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1531,"ΤΕΜ",1,"MC",1,"1FK70334CK711QG1"]
["1FK7033-4CK71-1QG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1531,"ΤΕΜ",1,"MC",1,"1FK70334CK711QG2"]
["1FK7033-4CK71-1QH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1667,"ΤΕΜ",1,"MC",1,"1FK70334CK711QH0"]
["1FK7033-4CK71-1QH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1767,"ΤΕΜ",1,"MC",1,"1FK70334CK711QH1"]
["1FK7033-4CK71-1QH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1767,"ΤΕΜ",1,"MC",1,"1FK70334CK711QH2"]
["1FK7033-4CK71-1RA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1934,"ΤΕΜ",1,"MC",1,"1FK70334CK711RA0"]
["1FK7033-4CK71-1RA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2034,"ΤΕΜ",1,"MC",1,"1FK70334CK711RA1"]
["1FK7033-4CK71-1RA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2034,"ΤΕΜ",1,"MC",1,"1FK70334CK711RA2"]
["1FK7033-4CK71-1RB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2173,"ΤΕΜ",1,"MC",1,"1FK70334CK711RB0"]
["1FK7033-4CK71-1RB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2273,"ΤΕΜ",1,"MC",1,"1FK70334CK711RB1"]
["1FK7033-4CK71-1RB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2273,"ΤΕΜ",1,"MC",1,"1FK70334CK711RB2"]
["1FK7033-4CK71-1RG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1839,"ΤΕΜ",1,"MC",1,"1FK70334CK711RG0"]
["1FK7033-4CK71-1RG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1940,"ΤΕΜ",1,"MC",1,"1FK70334CK711RG1"]
["1FK7033-4CK71-1RG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1940,"ΤΕΜ",1,"MC",1,"1FK70334CK711RG2"]
["1FK7033-4CK71-1RH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2076,"ΤΕΜ",1,"MC",1,"1FK70334CK711RH0"]
["1FK7033-4CK71-1RH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2176,"ΤΕΜ",1,"MC",1,"1FK70334CK711RH1"]
["1FK7033-4CK71-1RH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2176,"ΤΕΜ",1,"MC",1,"1FK70334CK711RH2"]
["1FK7033-4CK71-1UA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1412,"ΤΕΜ",1,"MC",1,"1FK70334CK711UA0"]
["1FK7033-4CK71-1UA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1512,"ΤΕΜ",1,"MC",1,"1FK70334CK711UA1"]
["1FK7033-4CK71-1UA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1512,"ΤΕΜ",1,"MC",1,"1FK70334CK711UA2"]
["1FK7033-4CK71-1UB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1651,"ΤΕΜ",1,"MC",1,"1FK70334CK711UB0"]
["1FK7033-4CK71-1UB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1752,"ΤΕΜ",1,"MC",1,"1FK70334CK711UB1"]
["1FK7033-4CK71-1UB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1752,"ΤΕΜ",1,"MC",1,"1FK70334CK711UB2"]
["1FK7033-4CK71-1UG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1318,"ΤΕΜ",1,"MC",1,"1FK70334CK711UG0"]
["1FK7033-4CK71-1UG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1418,"ΤΕΜ",1,"MC",1,"1FK70334CK711UG1"]
["1FK7033-4CK71-1UG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1418,"ΤΕΜ",1,"MC",1,"1FK70334CK711UG2"]
["1FK7033-4CK71-1UH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1554,"ΤΕΜ",1,"MC",1,"1FK70334CK711UH0"]
["1FK7033-4CK71-1UH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1655,"ΤΕΜ",1,"MC",1,"1FK70334CK711UH1"]
["1FK7033-4CK71-1UH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1655,"ΤΕΜ",1,"MC",1,"1FK70334CK711UH2"]
["1FK7033-4CK74-1AA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1789,"ΤΕΜ",1,"MC",1,"1FK70334CK741AA0"]
["1FK7033-4CK74-1AA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1889,"ΤΕΜ",1,"MC",1,"1FK70334CK741AA1"]
["1FK7033-4CK74-1AA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1889,"ΤΕΜ",1,"MC",1,"1FK70334CK741AA2"]
["1FK7033-4CK74-1AB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2028,"ΤΕΜ",1,"MC",1,"1FK70334CK741AB0"]
["1FK7033-4CK74-1AB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2129,"ΤΕΜ",1,"MC",1,"1FK70334CK741AB1"]
["1FK7033-4CK74-1AB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2129,"ΤΕΜ",1,"MC",1,"1FK70334CK741AB2"]
["1FK7033-4CK74-1AG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1695,"ΤΕΜ",1,"MC",1,"1FK70334CK741AG0"]
["1FK7033-4CK74-1AG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1795,"ΤΕΜ",1,"MC",1,"1FK70334CK741AG1"]
["1FK7033-4CK74-1AG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1795,"ΤΕΜ",1,"MC",1,"1FK70334CK741AG2"]
["1FK7033-4CK74-1AH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1931,"ΤΕΜ",1,"MC",1,"1FK70334CK741AH0"]
["1FK7033-4CK74-1AH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2032,"ΤΕΜ",1,"MC",1,"1FK70334CK741AH1"]
["1FK7033-4CK74-1AH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2032,"ΤΕΜ",1,"MC",1,"1FK70334CK741AH2"]
["1FK7033-4CK74-1EA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2195,"ΤΕΜ",1,"MC",1,"1FK70334CK741EA0"]
["1FK7033-4CK74-1EA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2295,"ΤΕΜ",1,"MC",1,"1FK70334CK741EA1"]
["1FK7033-4CK74-1EA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2295,"ΤΕΜ",1,"MC",1,"1FK70334CK741EA2"]
["1FK7033-4CK74-1EB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2434,"ΤΕΜ",1,"MC",1,"1FK70334CK741EB0"]
["1FK7033-4CK74-1EB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2535,"ΤΕΜ",1,"MC",1,"1FK70334CK741EB1"]
["1FK7033-4CK74-1EB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2535,"ΤΕΜ",1,"MC",1,"1FK70334CK741EB2"]
["1FK7033-4CK74-1EG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2101,"ΤΕΜ",1,"MC",1,"1FK70334CK741EG0"]
["1FK7033-4CK74-1EG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2201,"ΤΕΜ",1,"MC",1,"1FK70334CK741EG1"]
["1FK7033-4CK74-1EG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2201,"ΤΕΜ",1,"MC",1,"1FK70334CK741EG2"]
["1FK7033-4CK74-1EH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2338,"ΤΕΜ",1,"MC",1,"1FK70334CK741EH0"]
["1FK7033-4CK74-1EH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2438,"ΤΕΜ",1,"MC",1,"1FK70334CK741EH1"]
["1FK7033-4CK74-1EH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2438,"ΤΕΜ",1,"MC",1,"1FK70334CK741EH2"]
["1FK7033-4CK74-1SA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1149,"ΤΕΜ",1,"MC",1,"1FK70334CK741SA0"]
["1FK7033-4CK74-1SA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1249,"ΤΕΜ",1,"MC",1,"1FK70334CK741SA1"]
["1FK7033-4CK74-1SA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1249,"ΤΕΜ",1,"MC",1,"1FK70334CK741SA2"]
["1FK7033-4CK74-1SB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1388,"ΤΕΜ",1,"MC",1,"1FK70334CK741SB0"]
["1FK7033-4CK74-1SB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1488,"ΤΕΜ",1,"MC",1,"1FK70334CK741SB1"]
["1FK7033-4CK74-1SB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1488,"ΤΕΜ",1,"MC",1,"1FK70334CK741SB2"]
["1FK7033-4CK74-1SG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1054,"ΤΕΜ",1,"MC",1,"1FK70334CK741SG0"]
["1FK7033-4CK74-1SG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1155,"ΤΕΜ",1,"MC",1,"1FK70334CK741SG1"]
["1FK7033-4CK74-1SG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1155,"ΤΕΜ",1,"MC",1,"1FK70334CK741SG2"]
["1FK7033-4CK74-1SH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1291,"ΤΕΜ",1,"MC",1,"1FK70334CK741SH0"]
["1FK7033-4CK74-1SH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1391,"ΤΕΜ",1,"MC",1,"1FK70334CK741SH1"]
["1FK7033-4CK74-1SH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1391,"ΤΕΜ",1,"MC",1,"1FK70334CK741SH2"]
["1FK7033-4CK74-1TA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1149,"ΤΕΜ",1,"MC",1,"1FK70334CK741TA0"]
["1FK7033-4CK74-1TA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1249,"ΤΕΜ",1,"MC",1,"1FK70334CK741TA1"]
["1FK7033-4CK74-1TA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1249,"ΤΕΜ",1,"MC",1,"1FK70334CK741TA2"]
["1FK7033-4CK74-1TB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1388,"ΤΕΜ",1,"MC",1,"1FK70334CK741TB0"]
["1FK7033-4CK74-1TB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1488,"ΤΕΜ",1,"MC",1,"1FK70334CK741TB1"]
["1FK7033-4CK74-1TB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1488,"ΤΕΜ",1,"MC",1,"1FK70334CK741TB2"]
["1FK7033-4CK74-1TG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1054,"ΤΕΜ",1,"MC",1,"1FK70334CK741TG0"]
["1FK7033-4CK74-1TG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1155,"ΤΕΜ",1,"MC",1,"1FK70334CK741TG1"]
["1FK7033-4CK74-1TG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1155,"ΤΕΜ",1,"MC",1,"1FK70334CK741TG2"]
["1FK7033-4CK74-1TH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1291,"ΤΕΜ",1,"MC",1,"1FK70334CK741TH0"]
["1FK7033-4CK74-1TH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1391,"ΤΕΜ",1,"MC",1,"1FK70334CK741TH1"]
["1FK7033-4CK74-1TH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1391,"ΤΕΜ",1,"MC",1,"1FK70334CK741TH2"]
["1FK7034-2AF21-1BA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",2108,"ΤΕΜ",1,"MC",1,"1FK70342AF211BA0"]
["1FK7034-2AF21-1BA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",2210,"ΤΕΜ",1,"MC",1,"1FK70342AF211BA1"]
["1FK7034-2AF21-1BA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",2210,"ΤΕΜ",1,"MC",1,"1FK70342AF211BA2"]
["1FK7034-2AF21-1BB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",2347,"ΤΕΜ",1,"MC",1,"1FK70342AF211BB0"]
["1FK7034-2AF21-1BB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",2450,"ΤΕΜ",1,"MC",1,"1FK70342AF211BB1"]
["1FK7034-2AF21-1BB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",2450,"ΤΕΜ",1,"MC",1,"1FK70342AF211BB2"]
["1FK7034-2AF21-1BG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",2014,"ΤΕΜ",1,"MC",1,"1FK70342AF211BG0"]
["1FK7034-2AF21-1BG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",2116,"ΤΕΜ",1,"MC",1,"1FK70342AF211BG1"]
["1FK7034-2AF21-1BG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",2116,"ΤΕΜ",1,"MC",1,"1FK70342AF211BG2"]
["1FK7034-2AF21-1BH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",2250,"ΤΕΜ",1,"MC",1,"1FK70342AF211BH0"]
["1FK7034-2AF21-1BH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",2353,"ΤΕΜ",1,"MC",1,"1FK70342AF211BH1"]
["1FK7034-2AF21-1BH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65, DE flange IP67",2353,"ΤΕΜ",1,"MC",1,"1FK70342AF211BH2"]
["1FK7034-2AF21-1CA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12- bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",2512,"ΤΕΜ",1,"MC",1,"1FK70342AF211CA0"]
["1FK7034-2AF21-1CA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",2614,"ΤΕΜ",1,"MC",1,"1FK70342AF211CA1"]
["1FK7034-2AF21-1CA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",2614,"ΤΕΜ",1,"MC",1,"1FK70342AF211CA2"]
["1FK7034-2AF21-1CB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",2751,"ΤΕΜ",1,"MC",1,"1FK70342AF211CB0"]
["1FK7034-2AF21-1CB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",2853,"ΤΕΜ",1,"MC",1,"1FK70342AF211CB1"]
["1FK7034-2AF21-1CB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",2853,"ΤΕΜ",1,"MC",1,"1FK70342AF211CB2"]
["1FK7034-2AF21-1CG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",2417,"ΤΕΜ",1,"MC",1,"1FK70342AF211CG0"]
["1FK7034-2AF21-1CG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",2520,"ΤΕΜ",1,"MC",1,"1FK70342AF211CG1"]
["1FK7034-2AF21-1CG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",2520,"ΤΕΜ",1,"MC",1,"1FK70342AF211CG2"]
["1FK7034-2AF21-1CH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",2654,"ΤΕΜ",1,"MC",1,"1FK70342AF211CH0"]
["1FK7034-2AF21-1CH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",2756,"ΤΕΜ",1,"MC",1,"1FK70342AF211CH1"]
["1FK7034-2AF21-1CH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65, DE flange IP67",2756,"ΤΕΜ",1,"MC",1,"1FK70342AF211CH2"]
["1FK7034-2AF21-1DA1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2298,"ΤΕΜ",1,"MC",1,"1FK70342AF211DA1"]
["1FK7034-2AF21-1DA2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2298,"ΤΕΜ",1,"MC",1,"1FK70342AF211DA2"]
["1FK7034-2AF21-1DB1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2537,"ΤΕΜ",1,"MC",1,"1FK70342AF211DB1"]
["1FK7034-2AF21-1DG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2101,"ΤΕΜ",1,"MC",1,"1FK70342AF211DG0"]
["1FK7034-2AF21-1DG2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2204,"ΤΕΜ",1,"MC",1,"1FK70342AF211DG2"]
["1FK7034-2AF21-1DH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2338,"ΤΕΜ",1,"MC",1,"1FK70342AF211DH0"]
["1FK7034-2AF21-1FB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2839,"ΤΕΜ",1,"MC",1,"1FK70342AF211FB0"]
["1FK7034-2AF21-1FB2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2941,"ΤΕΜ",1,"MC",1,"1FK70342AF211FB2"]
["1FK7034-2AF21-1FG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2505,"ΤΕΜ",1,"MC",1,"1FK70342AF211FG0"]
["1FK7034-2AF21-1FG2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2607,"ΤΕΜ",1,"MC",1,"1FK70342AF211FG2"]
["1FK7034-2AF21-1FH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2742,"ΤΕΜ",1,"MC",1,"1FK70342AF211FH0"]
["1FK7034-2AF21-1FH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2844,"ΤΕΜ",1,"MC",1,"1FK70342AF211FH2"]
["1FK7034-2AF21-1PA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP64",1468,"ΤΕΜ",1,"MC",1,"1FK70342AF211PA0"]
["1FK7034-2AF21-1PA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP65",1570,"ΤΕΜ",1,"MC",1,"1FK70342AF211PA1"]
["1FK7034-2AF21-1PA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1570,"ΤΕΜ",1,"MC",1,"1FK70342AF211PA2"]
["1FK7034-2AF21-1PB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP64",1707,"ΤΕΜ",1,"MC",1,"1FK70342AF211PB0"]
["1FK7034-2AF21-1PB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP65",1809,"ΤΕΜ",1,"MC",1,"1FK70342AF211PB1"]
["1FK7034-2AF21-1PB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1809,"ΤΕΜ",1,"MC",1,"1FK70342AF211PB2"]
["1FK7034-2AF21-1PG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP64",1373,"ΤΕΜ",1,"MC",1,"1FK70342AF211PG0"]
["1FK7034-2AF21-1PG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP65",1476,"ΤΕΜ",1,"MC",1,"1FK70342AF211PG1"]
["1FK7034-2AF21-1PG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1476,"ΤΕΜ",1,"MC",1,"1FK70342AF211PG2"]
["1FK7034-2AF21-1PH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP64",1610,"ΤΕΜ",1,"MC",1,"1FK70342AF211PH0"]
["1FK7034-2AF21-1PH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP65",1712,"ΤΕΜ",1,"MC",1,"1FK70342AF211PH1"]
["1FK7034-2AF21-1PH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1712,"ΤΕΜ",1,"MC",1,"1FK70342AF211PH2"]
["1FK7034-2AF21-1QA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",1580,"ΤΕΜ",1,"MC",1,"1FK70342AF211QA0"]
["1FK7034-2AF21-1QA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",1682,"ΤΕΜ",1,"MC",1,"1FK70342AF211QA1"]
["1FK7034-2AF21-1QA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1682,"ΤΕΜ",1,"MC",1,"1FK70342AF211QA2"]
["1FK7034-2AF21-1QB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",1820,"ΤΕΜ",1,"MC",1,"1FK70342AF211QB0"]
["1FK7034-2AF21-1QB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",1922,"ΤΕΜ",1,"MC",1,"1FK70342AF211QB1"]
["1FK7034-2AF21-1QB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",1922,"ΤΕΜ",1,"MC",1,"1FK70342AF211QB2"]
["1FK7034-2AF21-1QG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",1486,"ΤΕΜ",1,"MC",1,"1FK70342AF211QG0"]
["1FK7034-2AF21-1QG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",1588,"ΤΕΜ",1,"MC",1,"1FK70342AF211QG1"]
["1FK7034-2AF21-1QG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",1588,"ΤΕΜ",1,"MC",1,"1FK70342AF211QG2"]
["1FK7034-2AF21-1QH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",1723,"ΤΕΜ",1,"MC",1,"1FK70342AF211QH0"]
["1FK7034-2AF21-1QH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",1825,"ΤΕΜ",1,"MC",1,"1FK70342AF211QH1"]
["1FK7034-2AF21-1QH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65, DE flange IP67",1825,"ΤΕΜ",1,"MC",1,"1FK70342AF211QH2"]
["1FK7034-2AF21-1RA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",1989,"ΤΕΜ",1,"MC",1,"1FK70342AF211RA0"]
["1FK7034-2AF21-1RA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",2091,"ΤΕΜ",1,"MC",1,"1FK70342AF211RA1"]
["1FK7034-2AF21-1RA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",2091,"ΤΕΜ",1,"MC",1,"1FK70342AF211RA2"]
["1FK7034-2AF21-1RB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",2228,"ΤΕΜ",1,"MC",1,"1FK70342AF211RB0"]
["1FK7034-2AF21-1RB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",2331,"ΤΕΜ",1,"MC",1,"1FK70342AF211RB1"]
["1FK7034-2AF21-1RB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",2331,"ΤΕΜ",1,"MC",1,"1FK70342AF211RB2"]
["1FK7034-2AF21-1RG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",1895,"ΤΕΜ",1,"MC",1,"1FK70342AF211RG0"]
["1FK7034-2AF21-1RG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",1997,"ΤΕΜ",1,"MC",1,"1FK70342AF211RG1"]
["1FK7034-2AF21-1RG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",1997,"ΤΕΜ",1,"MC",1,"1FK70342AF211RG2"]
["1FK7034-2AF21-1RH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",2131,"ΤΕΜ",1,"MC",1,"1FK70342AF211RH0"]
["1FK7034-2AF21-1RH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",2234,"ΤΕΜ",1,"MC",1,"1FK70342AF211RH1"]
["1FK7034-2AF21-1RH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65, DE flange IP67",2234,"ΤΕΜ",1,"MC",1,"1FK70342AF211RH2"]
["1FK7034-2AF21-1UA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP64",1468,"ΤΕΜ",1,"MC",1,"1FK70342AF211UA0"]
["1FK7034-2AF21-1UA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP65",1570,"ΤΕΜ",1,"MC",1,"1FK70342AF211UA1"]
["1FK7034-2AF21-1UA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1570,"ΤΕΜ",1,"MC",1,"1FK70342AF211UA2"]
["1FK7034-2AF21-1UB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP64",1707,"ΤΕΜ",1,"MC",1,"1FK70342AF211UB0"]
["1FK7034-2AF21-1UB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP65",1809,"ΤΕΜ",1,"MC",1,"1FK70342AF211UB1"]
["1FK7034-2AF21-1UB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1809,"ΤΕΜ",1,"MC",1,"1FK70342AF211UB2"]
["1FK7034-2AF21-1UG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP64",1373,"ΤΕΜ",1,"MC",1,"1FK70342AF211UG0"]
["1FK7034-2AF21-1UG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP65",1476,"ΤΕΜ",1,"MC",1,"1FK70342AF211UG1"]
["1FK7034-2AF21-1UG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1476,"ΤΕΜ",1,"MC",1,"1FK70342AF211UG2"]
["1FK7034-2AF21-1UH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP64",1610,"ΤΕΜ",1,"MC",1,"1FK70342AF211UH0"]
["1FK7034-2AF21-1UH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP65",1712,"ΤΕΜ",1,"MC",1,"1FK70342AF211UH1"]
["1FK7034-2AF21-1UH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1712,"ΤΕΜ",1,"MC",1,"1FK70342AF211UH2"]
["1FK7034-2AF24-1EG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2156,"ΤΕΜ",1,"MC",1,"1FK70342AF241EG0"]
["1FK7034-2AF24-1SA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP64",1204,"ΤΕΜ",1,"MC",1,"1FK70342AF241SA0"]
["1FK7034-2AF24-1SA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP65",1306,"ΤΕΜ",1,"MC",1,"1FK70342AF241SA1"]
["1FK7034-2AF24-1SA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1306,"ΤΕΜ",1,"MC",1,"1FK70342AF241SA2"]
["1FK7034-2AF24-1SB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP64",1443,"ΤΕΜ",1,"MC",1,"1FK70342AF241SB0"]
["1FK7034-2AF24-1SB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP65",1546,"ΤΕΜ",1,"MC",1,"1FK70342AF241SB1"]
["1FK7034-2AF24-1SB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",1546,"ΤΕΜ",1,"MC",1,"1FK70342AF241SB2"]
["1FK7034-2AF24-1SG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP64",1110,"ΤΕΜ",1,"MC",1,"1FK70342AF241SG0"]
["1FK7034-2AF24-1SG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP65",1212,"ΤΕΜ",1,"MC",1,"1FK70342AF241SG1"]
["1FK7034-2AF24-1SG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP65 DE flange IP67",1212,"ΤΕΜ",1,"MC",1,"1FK70342AF241SG2"]
["1FK7034-2AF24-1SH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, type of protection IP64",1347,"ΤΕΜ",1,"MC",1,"1FK70342AF241SH0"]
["1FK7034-2AF24-1SH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, type of protection IP65",1449,"ΤΕΜ",1,"MC",1,"1FK70342AF241SH1"]
["1FK7034-2AF24-1SH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, degree of protection IP65 DE Flange IP67",1449,"ΤΕΜ",1,"MC",1,"1FK70342AF241SH2"]
["1FK7034-2AF24-1TA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP64",1204,"ΤΕΜ",1,"MC",1,"1FK70342AF241TA0"]
["1FK7034-2AF24-1TA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP65",1306,"ΤΕΜ",1,"MC",1,"1FK70342AF241TA1"]
["1FK7034-2AF24-1TA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1306,"ΤΕΜ",1,"MC",1,"1FK70342AF241TA2"]
["1FK7034-2AF24-1TB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP64",1443,"ΤΕΜ",1,"MC",1,"1FK70342AF241TB0"]
["1FK7034-2AF24-1TB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP65",1546,"ΤΕΜ",1,"MC",1,"1FK70342AF241TB1"]
["1FK7034-2AF24-1TB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",1546,"ΤΕΜ",1,"MC",1,"1FK70342AF241TB2"]
["1FK7034-2AF24-1TG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP64",1110,"ΤΕΜ",1,"MC",1,"1FK70342AF241TG0"]
["1FK7034-2AF24-1TG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP65",1212,"ΤΕΜ",1,"MC",1,"1FK70342AF241TG1"]
["1FK7034-2AF24-1TG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP65 DE flange IP67",1212,"ΤΕΜ",1,"MC",1,"1FK70342AF241TG2"]
["1FK7034-2AF24-1TH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, type of protection IP64",1347,"ΤΕΜ",1,"MC",1,"1FK70342AF241TH0"]
["1FK7034-2AF24-1TH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, type of protection IP65",1449,"ΤΕΜ",1,"MC",1,"1FK70342AF241TH1"]
["1FK7034-2AF24-1TH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, degree of protection IP65 DE Flange IP67",1449,"ΤΕΜ",1,"MC",1,"1FK70342AF241TH2"]
["1FK7034-2AK71-1BA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) shaft with feather key, Tolerance N without holding brake Degree of protection IP64",2108,"ΤΕΜ",1,"MC",1,"1FK70342AK711BA0"]
["1FK7034-2AK71-1BA1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) shaft with feather key, Tolerance N without holding brake Degree of protection IP65",2210,"ΤΕΜ",1,"MC",1,"1FK70342AK711BA1"]
["1FK7034-2AK71-1BA2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) shaft with feather key, Tolerance N without holding brake Degree of protection IP65 DE flange IP67",2210,"ΤΕΜ",1,"MC",1,"1FK70342AK711BA2"]
["1FK7034-2AK71-1BB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) shaft with feather key, Tolerance N with holding brake Degree of protection IP64",2347,"ΤΕΜ",1,"MC",1,"1FK70342AK711BB0"]
["1FK7034-2AK71-1BB1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) shaft with feather key, Tolerance N with holding brake Degree of protection IP65",2450,"ΤΕΜ",1,"MC",1,"1FK70342AK711BB1"]
["1FK7034-2AK71-1BB2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) shaft with feather key, Tolerance N with holding brake Degree of protection IP65 DE flange IP67",2450,"ΤΕΜ",1,"MC",1,"1FK70342AK711BB2"]
["1FK7034-2AK71-1BG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) smooth shaft, Tolerance N without holding brake Degree of protection IP64",2014,"ΤΕΜ",1,"MC",1,"1FK70342AK711BG0"]
["1FK7034-2AK71-1BG1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) smooth shaft, Tolerance N without holding brake Degree of protection IP65",2116,"ΤΕΜ",1,"MC",1,"1FK70342AK711BG1"]
["1FK7034-2AK71-1BG2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) smooth shaft, Tolerance N without holding brake Degree of protection IP65 DE flange IP67",2116,"ΤΕΜ",1,"MC",1,"1FK70342AK711BG2"]
["1FK7034-2AK71-1BH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) smooth shaft, Tolerance N with holding brake Degree of protection IP64",2250,"ΤΕΜ",1,"MC",1,"1FK70342AK711BH0"]
["1FK7034-2AK71-1BH1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) smooth shaft, Tolerance N with holding brake Degree of protection IP65",2353,"ΤΕΜ",1,"MC",1,"1FK70342AK711BH1"]
["1FK7034-2AK71-1BH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) smooth shaft, Tolerance N with holding brake Degree of protection IP65 DE flange IP67",2353,"ΤΕΜ",1,"MC",1,"1FK70342AK711BH2"]
["1FK7034-2AK71-1CA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM24DQI) shaft with feather key, Tolerance N without holding brake Degree of protection IP64",2512,"ΤΕΜ",1,"MC",1,"1FK70342AK711CA0"]
["1FK7034-2AK71-1CA1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM24DQI) shaft with feather key, Tolerance N without holding brake Degree of protection IP65",2614,"ΤΕΜ",1,"MC",1,"1FK70342AK711CA1"]
["1FK7034-2AK71-1CA2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM24DQI) shaft with feather key, Tolerance N without holding brake Degree of protection IP65 DE flange IP67",2614,"ΤΕΜ",1,"MC",1,"1FK70342AK711CA2"]
["1FK7034-2AK71-1CB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM24DQI) shaft with feather key, Tolerance N with holding brake Degree of protection IP64",2751,"ΤΕΜ",1,"MC",1,"1FK70342AK711CB0"]
["1FK7034-2AK71-1CB1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM24DQI) shaft with feather key, Tolerance N with holding brake Degree of protection IP65",2853,"ΤΕΜ",1,"MC",1,"1FK70342AK711CB1"]
["1FK7034-2AK71-1CB2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM24DQI) shaft with feather key, Tolerance N with holding brake Degree of protection IP65 DE flange IP67",2853,"ΤΕΜ",1,"MC",1,"1FK70342AK711CB2"]
["1FK7034-2AK71-1CG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM24DQI) smooth shaft, Tolerance N without holding brake Degree of protection IP64",2417,"ΤΕΜ",1,"MC",1,"1FK70342AK711CG0"]
["1FK7034-2AK71-1CG1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM24DQI) smooth shaft, Tolerance N without holding brake Degree of protection IP65",2520,"ΤΕΜ",1,"MC",1,"1FK70342AK711CG1"]
["1FK7034-2AK71-1CG2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM24DQI) smooth shaft, Tolerance N without holding brake Degree of protection IP65 DE flange IP67",2520,"ΤΕΜ",1,"MC",1,"1FK70342AK711CG2"]
["1FK7034-2AK71-1CH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM24DQI) smooth shaft, Tolerance N with holding brake Degree of protection IP64",2654,"ΤΕΜ",1,"MC",1,"1FK70342AK711CH0"]
["1FK7034-2AK71-1CH1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM24DQI) smooth shaft, Tolerance N with holding brake Degree of protection IP65",2756,"ΤΕΜ",1,"MC",1,"1FK70342AK711CH1"]
["1FK7034-2AK71-1CH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM24DQI) smooth shaft, Tolerance N with holding brake Degree of protection IP65 DE flange IP67",2756,"ΤΕΜ",1,"MC",1,"1FK70342AK711CH2"]
["1FK7034-2AK71-1DA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2196,"ΤΕΜ",1,"MC",1,"1FK70342AK711DA0"]
["1FK7034-2AK71-1DA1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2296,"ΤΕΜ",1,"MC",1,"1FK70342AK711DA1"]
["1FK7034-2AK71-1DB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2435,"ΤΕΜ",1,"MC",1,"1FK70342AK711DB0"]
["1FK7034-2AK71-1DG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2101,"ΤΕΜ",1,"MC",1,"1FK70342AK711DG0"]
["1FK7034-2AK71-1DG1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2202,"ΤΕΜ",1,"MC",1,"1FK70342AK711DG1"]
["1FK7034-2AK71-1DH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2338,"ΤΕΜ",1,"MC",1,"1FK70342AK711DH0"]
["1FK7034-2AK71-1DH1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2438,"ΤΕΜ",1,"MC",1,"1FK70342AK711DH1"]
["1FK7034-2AK71-1FA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2599,"ΤΕΜ",1,"MC",1,"1FK70342AK711FA0"]
["1FK7034-2AK71-1FA1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2700,"ΤΕΜ",1,"MC",1,"1FK70342AK711FA1"]
["1FK7034-2AK71-1FB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2839,"ΤΕΜ",1,"MC",1,"1FK70342AK711FB0"]
["1FK7034-2AK71-1FB1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2939,"ΤΕΜ",1,"MC",1,"1FK70342AK711FB1"]
["1FK7034-2AK71-1FG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2505,"ΤΕΜ",1,"MC",1,"1FK70342AK711FG0"]
["1FK7034-2AK71-1FG1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2605,"ΤΕΜ",1,"MC",1,"1FK70342AK711FG1"]
["1FK7034-2AK71-1FG2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2605,"ΤΕΜ",1,"MC",1,"1FK70342AK711FG2"]
["1FK7034-2AK71-1FH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2742,"ΤΕΜ",1,"MC",1,"1FK70342AK711FH0"]
["1FK7034-2AK71-1FH1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2842,"ΤΕΜ",1,"MC",1,"1FK70342AK711FH1"]
["1FK7034-2AK71-1FH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2842,"ΤΕΜ",1,"MC",1,"1FK70342AK711FH2"]
["1FK7034-2AK71-1PA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.63 kW; UDC=600V M0=1.6 Nm (100K); NN=6000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP64",1468,"ΤΕΜ",1,"MC",1,"1FK70342AK711PA0"]
["1FK7034-2AK71-1PA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.63 kW; UDC=600V M0=1.6 Nm (100K); NN=6000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP65",1570,"ΤΕΜ",1,"MC",1,"1FK70342AK711PA1"]
["1FK7034-2AK71-1PA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.63 kW; UDC=600V M0=1.6 Nm (100K); NN=6000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1570,"ΤΕΜ",1,"MC",1,"1FK70342AK711PA2"]
["1FK7034-2AK71-1PB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.63 kW; UDC=600V M0=1.6 Nm (100K); NN=6000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP64",1707,"ΤΕΜ",1,"MC",1,"1FK70342AK711PB0"]
["1FK7034-2AK71-1PB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.63 kW; UDC=600V M0=1.6 Nm (100K); NN=6000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP65",1809,"ΤΕΜ",1,"MC",1,"1FK70342AK711PB1"]
["1FK7034-2AK71-1PB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.63 kW; UDC=600V M0=1.6 Nm (100K); NN=6000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1809,"ΤΕΜ",1,"MC",1,"1FK70342AK711PB2"]
["1FK7034-2AK71-1PG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.63 kW; UDC=600V M0=1.6 Nm (100K); NN=6000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP64",1373,"ΤΕΜ",1,"MC",1,"1FK70342AK711PG0"]
["1FK7034-2AK71-1PG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.63 kW; UDC=600V M0=1.6 Nm (100K); NN=6000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP65",1476,"ΤΕΜ",1,"MC",1,"1FK70342AK711PG1"]
["1FK7034-2AK71-1PG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.63 kW; UDC=600V M0=1.6 Nm (100K); NN=6000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1476,"ΤΕΜ",1,"MC",1,"1FK70342AK711PG2"]
["1FK7034-2AK71-1PH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.63 kW; UDC=600V M0=1.6 Nm (100K); NN=6000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP64",1610,"ΤΕΜ",1,"MC",1,"1FK70342AK711PH0"]
["1FK7034-2AK71-1PH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.63 kW; UDC=600V M0=1.6 Nm (100K); NN=6000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP65",1712,"ΤΕΜ",1,"MC",1,"1FK70342AK711PH1"]
["1FK7034-2AK71-1PH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.63 kW; UDC=600V M0=1.6 Nm (100K); NN=6000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1712,"ΤΕΜ",1,"MC",1,"1FK70342AK711PH2"]
["1FK7034-2AK71-1QA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) shaft with feather key, Tolerance N without holding brake Degree of protection IP64",1580,"ΤΕΜ",1,"MC",1,"1FK70342AK711QA0"]
["1FK7034-2AK71-1QA1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) shaft with feather key, Tolerance N without holding brake Degree of protection IP65",1682,"ΤΕΜ",1,"MC",1,"1FK70342AK711QA1"]
["1FK7034-2AK71-1QA2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) shaft with feather key, Tolerance N without holding brake Degree of protection IP65 DE flange IP67",1682,"ΤΕΜ",1,"MC",1,"1FK70342AK711QA2"]
["1FK7034-2AK71-1QB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) shaft with feather key, Tolerance N with holding brake Degree of protection IP64",1820,"ΤΕΜ",1,"MC",1,"1FK70342AK711QB0"]
["1FK7034-2AK71-1QB1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) shaft with feather key, Tolerance N with holding brake Degree of protection IP65",1922,"ΤΕΜ",1,"MC",1,"1FK70342AK711QB1"]
["1FK7034-2AK71-1QB2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) shaft with feather key, Tolerance N with holding brake Degree of protection IP65 DE flange IP67",1922,"ΤΕΜ",1,"MC",1,"1FK70342AK711QB2"]
["1FK7034-2AK71-1QG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) smooth shaft, Tolerance N without holding brake Degree of protection IP64",1486,"ΤΕΜ",1,"MC",1,"1FK70342AK711QG0"]
["1FK7034-2AK71-1QG1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) smooth shaft, Tolerance N without holding brake Degree of protection IP65",1588,"ΤΕΜ",1,"MC",1,"1FK70342AK711QG1"]
["1FK7034-2AK71-1QG2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) smooth shaft, Tolerance N without holding brake Degree of protection IP65 DE flange IP67",1588,"ΤΕΜ",1,"MC",1,"1FK70342AK711QG2"]
["1FK7034-2AK71-1QH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) smooth shaft, Tolerance N with holding brake Degree of protection IP64",1723,"ΤΕΜ",1,"MC",1,"1FK70342AK711QH0"]
["1FK7034-2AK71-1QH1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) smooth shaft, Tolerance N with holding brake Degree of protection IP65",1825,"ΤΕΜ",1,"MC",1,"1FK70342AK711QH1"]
["1FK7034-2AK74-1AG2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1851,"ΤΕΜ",1,"MC",1,"1FK70342AK741AG2"]
["1FK7040-2AK71-1DH1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.69kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2451,"ΤΕΜ",1,"MC",1,"1FK70402AK711DH1"]
["1FK7040-2AK74-1SA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.69 kW; UDC=600V M0=1.6 Nm (100K); NN=6000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=4) shaft with feather key, tolerance N without holding brake degree of protection IP64",1170,"ΤΕΜ",1,"MC",1,"1FK70402AK741SA0"]
["1FK7042-2AC71-1RB1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.59kW; UDC=600V M0=3Nm (100K); NN=2000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 20-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake IP65 degree of protection",2413,"ΤΕΜ",1,"MC",1,"1FK70422AC711RB1"]
["1FK7042-2AF21-1RA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.82 kW; UDC=300 V M0=3 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 20-bit +12- bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65 DE flange IP67",2128,"ΤΕΜ",1,"MC",1,"1FK70422AF211RA2"]
["1FK7042-2AF71-1FA1","SIMOTICS S SIMOTICS S-1FK7 Synchronous motor 1FK7-CT PN=0.82kW; UDC=600V M0=3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2736,"ΤΕΜ",1,"MC",1,"1FK70422AF711FA1"]
["1FK7042-2AF74-1AG1","SIMOTICS S SIMOTICS S-1FK7 Synchronous motor 1FK7-CT PN=0.82kW; UDC=600V M0=3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1887,"ΤΕΜ",1,"MC",1,"1FK70422AF741AG1"]
["1FK7042-2AK71-1CB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.94kW; UDC=600V M0=3Nm (100K); NN=6000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake IP64 degree of protection",2833,"ΤΕΜ",1,"MC",1,"1FK70422AK711CB0"]
["1FK7042-2AK74-1TG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.94 kW; UDC=600V M0=3Nm (100K); NN=6000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP65 DE flange IP67",1248,"ΤΕΜ",1,"MC",1,"1FK70422AK741TG2"]
["1FK7042-3BK71-1CB1","SIMOTICS S synchronous motor 1FK7-HI PN=0.94 kW; UDC=600 V M0=3 Nm (100K); NN=6000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12- bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",2935,"ΤΕΜ",1,"MC",1,"1FK70423BK711CB1"]
["1FK7043-4CF21-1QA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.94kW; UDC=300V; M0=3. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1665,"ΤΕΜ",1,"MC",1,"1FK70434CF211QA0"]
["1FK7043-4CH74-1AA1","SIMOTICS S Synchronous motor 1FK7-HD PN=1.2kW; UDC=600V M0=3.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2029,"ΤΕΜ",1,"MC",1,"1FK70434CH741AA1"]
["1FK7043-4CK71-1BH2","SIMOTICS S Synchronous motor 1FK7-HD PN=1.3kW; UDC=600V M0=3.5Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2481,"ΤΕΜ",1,"MC",1,"1FK70434CK711BH2"]
["1FK7043-4CK74-1TB0","SIMOTICS S Synchronous motor 1FK7-HD PN=1.3kW; UDC=600V M0=3.5Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1574,"ΤΕΜ",1,"MC",1,"1FK70434CK741TB0"]
["1FK7044-4CF71-1PA0","SIMOTICS S Synchronous motor 1FK7-HD PN=1.2kW; UDC=600V M0=4.5Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1630,"ΤΕΜ",1,"MC",1,"1FK70444CF711PA0"]
["1FK7044-4CH71-1PB0","SIMOTICS S Synchronous motor 1FK7-HD PN=1.4kW; UDC=600V M0=4.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1915,"ΤΕΜ",1,"MC",1,"1FK70444CH711PB0"]
["1FK7044-4CH71-1QA2","SIMOTICS S Synchronous motor 1FK7-HD PN=1.4kW; UDC=600V M0=4.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1842,"ΤΕΜ",1,"MC",1,"1FK70444CH711QA2"]
["1FK7044-4CH74-1TH2","SIMOTICS S Synchronous motor 1FK7-HD PN=1.4kW; UDC=600V M0=4.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1655,"ΤΕΜ",1,"MC",1,"1FK70444CH741TH2"]
["1FK7060-2AC74-1AH1","SIMOTICS S Synchronous motor 1FK7-CT PN=1.1kW; UDC=600V M0=6Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2455,"ΤΕΜ",1,"MC",1,"1FK70602AC741AH1"]
["1FK7060-2AF71-1RA0","SIMOTICS S synchronous motor 1FK7-CT PN=1.5kW; UDC=600V M0=6Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 20-bit + 12-bit multiturn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake, degree of protection IP64",2260,"ΤΕΜ",1,"MC",1,"1FK70602AF711RA0"]
["1FK7060-2AF74-1TB1","SIMOTICS S synchronous motor 1FK7-CT PN=1.5 kW; UDC=600V M0=6Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP65",1908,"ΤΕΜ",1,"MC",1,"1FK70602AF741TB1"]
["1FK7060-2AH71-1RB0","SIMOTICS S synchronous motor 1FK7-CT PN=1.7 kW; UDC=600 V M0=6 Nm (100K); NN=4500 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 20-bit +12- bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",2591,"ΤΕΜ",1,"MC",1,"1FK70602AH711RB0"]
["1FK7060-3BF71-1FG1","SIMOTICS S Synchronous motor 1FK7-HI PN=1.5kW; UDC=600V M0=6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2876,"ΤΕΜ",1,"MC",1,"1FK70603BF711FG1"]
["1FK7060-3BF74-1AH1","SIMOTICS S Synchronous motor 1FK7-HI PN=1.5kW; UDC=600V M0=6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VP 2048 S/R WITH C- AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2455,"ΤΕΜ",1,"MC",1,"1FK70603BF741AH1"]
["1FK7061-4CF74-1TB1","SIMOTICS S Synchronous motor 1FK7-HD PN=1.7kW; UDC=600V M0=6.4Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2027,"ΤΕΜ",1,"MC",1,"1FK70614CF741TB1"]
["1FK7061-4CH74-1EH1","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=6.4Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2982,"ΤΕΜ",1,"MC",1,"1FK70614CH741EH1"]
["1FK7062-2AC71-1DB0","SIMOTICS S Synchronous motor 1FK7-CT PN=1.5kW; UDC=600V M0=8.5Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2939,"ΤΕΜ",1,"MC",1,"1FK70622AC711DB0"]
["1FK7062-2AC71-1RB1","SIMOTICS S synchronous motor 1FK7-CT PN=1.5kW; UDC=600V M0=8.5Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 20-bit + 12-bit multiturn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake, degree of protection IP65",2835,"ΤΕΜ",1,"MC",1,"1FK70622AC711RB1"]
["1FK7062-2AF71-1FA1","SIMOTICS S Synchronous motor 1FK7-CT PN=1.9kW; UDC=600V M0=8.5Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",3114,"ΤΕΜ",1,"MC",1,"1FK70622AF711FA1"]
["1FK7062-2AF74-1EH1","SIMOTICS S Synchronous motor 1FK7-CT PN=1.9kW; UDC=600V M0=8.5Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",3005,"ΤΕΜ",1,"MC",1,"1FK70622AF741EH1"]
["1FK7062-2AH71-1UH1","SIMOTICS S synchronous motor 1FK7-CT PN=1.4 kW; UDC=600V M0=8.5Nm (100K); NN=4500rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP65",2222,"ΤΕΜ",1,"MC",1,"1FK70622AH711UH1"]
["1FK7062-3BF71-1RH0","SIMOTICS S synchronous motor 1FK7-HI PN=1.9 kW; UDC=600 V M0=8.5 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 20-bit +12- bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",2641,"ΤΕΜ",1,"MC",1,"1FK70623BF711RH0"]
["1FK7063-2AC71-1FH0","SIMOTICS S Synchronous motor 1FK7-CT PN=1.9kW; UDC=600V M0=11Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3353,"ΤΕΜ",1,"MC",1,"1FK70632AC711FH0"]
["1FK7063-2AC74-1SA1","SIMOTICS S synchronous motor 1FK7-CT PN=1.9 kW; UDC=600V M0=11 Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=4) shaft with feather key, tolerance N without holding brake degree of protection IP65",1821,"ΤΕΜ",1,"MC",1,"1FK70632AC741SA1"]
["1FK7063-2AF71-1DA2","SIMOTICS S Synchronous motor 1FK7-CT PN=2.3kW; UDC=600V M0=11Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2811,"ΤΕΜ",1,"MC",1,"1FK70632AF711DA2"]
["1FK7063-2AF74-1EG2","SIMOTICS S Synchronous motor 1FK7-CT PN=2.3kW; UDC=600V M0=11Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2771,"ΤΕΜ",1,"MC",1,"1FK70632AF741EG2"]
["1FK7063-2AH71-1RA0","SIMOTICS S synchronous motor 1FK7-CT PN=1.4 kW; UDC=600 V M0=11 Nm (100K); NN=4500 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 20-bit +12- bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",2504,"ΤΕΜ",1,"MC",1,"1FK70632AH711RA0"]
["1FK7063-2AH74-1TH1","SIMOTICS S synchronous motor 1FK7-CT PN=1.4 kW; UDC=600V M0=11 Nm (100K); NN=4500rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, type of protection IP65",2061,"ΤΕΜ",1,"MC",1,"1FK70632AH741TH1"]
["1FK7064-4CF71-1BH1","SIMOTICS S Synchronous motor 1FK7-HD PN=2.5kW; UDC=600V M0=12Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3136,"ΤΕΜ",1,"MC",1,"1FK70644CF711BH1"]
["1FK7064-4CF74-1AA2","SIMOTICS S Synchronous motor 1FK7-HD PN=2.5kW; UDC=600V M0=12Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2634,"ΤΕΜ",1,"MC",1,"1FK70644CF741AA2"]
["1FK7064-4CH71-1CG2","SIMOTICS S Synchronous motor 1FK7-HD PN=2.4kW; UDC=600V M0=12Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",3206,"ΤΕΜ",1,"MC",1,"1FK70644CH711CG2"]
["1FK7080-2AF71-1BA2","SIMOTICS S synchronous motor 1FK7-CT PN=2.1 kW; UDC=600 V M0=8 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65 DE flange IP67",2667,"ΤΕΜ",1,"MC",1,"1FK70802AF711BA2"]
["1FK7080-2AF71-1UA0","SIMOTICS S synchronous motor 1FK7-CT PN=2.1 kW; UDC=600 V M0=8 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake degree of protection IP64",1924,"ΤΕΜ",1,"MC",1,"1FK70802AF711UA0"]
["1FK7080-2AH71-1RA0","SIMOTICS S synchronous motor 1FK7-CT PN=2.1 kW; UDC=600 V M0=8 Nm (100K); NN=4500 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 20-bit +12- bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",2446,"ΤΕΜ",1,"MC",1,"1FK70802AH711RA0"]
["1FK7080-2AH71-1UA0","SIMOTICS S synchronous motor 1FK7-CT PN=2.1 kW; UDC=600 V M0=8 Nm (100K); NN=4500 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake degree of protection IP64",1924,"ΤΕΜ",1,"MC",1,"1FK70802AH711UA0"]
["1FK7081-2AC71-1RG2","SIMOTICS S synchronous motor 1FK7-CT PN=2.1 kW; UDC=600V M0=12Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",2692,"ΤΕΜ",1,"MC",1,"1FK70812AC711RG2"]
["1FK7081-2AC74-1SG2","SIMOTICS S synchronous motor 1FK7-CT PN=2.1 kW; UDC=600V M0=12Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=4) smooth shaft, tolerance N without holding brake, type of protection IP65 DE flange IP67",1907,"ΤΕΜ",1,"MC",1,"1FK70812AC741SG2"]
["1FK7081-2AF71-1UG2","SIMOTICS S synchronous motor 1FK7-CT PN=2.7 kW; UDC=600 V M0=12 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake degree of protection IP65 DE flange IP67",2170,"ΤΕΜ",1,"MC",1,"1FK70812AF711UG2"]
["1FK7081-2AH71-1PA1","SIMOTICS S synchronous motor 1FK7-CT PN=1.8 kW; UDC=600V M0=12Nm (100K); NN=4500rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP65",2264,"ΤΕΜ",1,"MC",1,"1FK70812AH711PA1"]
["1FK7081-3BF71-1BG1","SIMOTICS S synchronous motor 1FK7-HI PN=2.7kW; UDC=600V M0=12Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) Smooth shaft, tolerance N without holding brake, degree of protection IP65",2811,"ΤΕΜ",1,"MC",1,"1FK70813BF711BG1"]
["1FK7083-2AC71-1CH1","SIMOTICS S synchronous motor 1FK7-CT PN=2.6kW; UDC=600V M0=16Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit + 12-bit multiturn with DRIVE-CLiQ interface (encoder AM24DQI) Smooth shaft, tolerance N with holding brake, degree of protection IP65",3781,"ΤΕΜ",1,"MC",1,"1FK70832AC711CH1"]
["1FK7083-2AC74-1AH1","SIMOTICS S Synchronous motor 1FK7-CT PN=2.6kW; UDC=600V M0=16Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3112,"ΤΕΜ",1,"MC",1,"1FK70832AC741AH1"]
["1FK7083-2AF71-1DH1","SIMOTICS S Synchronous motor 1FK7-CT PN=3.3kW; UDC=600V M0=16Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3463,"ΤΕΜ",1,"MC",1,"1FK70832AF711DH1"]
["1FK7083-2AF74-1TB2","SIMOTICS S synchronous motor 1FK7-CT PN=3.3 kW; UDC=600V M0=16 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",2568,"ΤΕΜ",1,"MC",1,"1FK70832AF741TB2"]
["1FK7083-2AH71-1DG1","SIMOTICS S Synchronous motor 1FK7-CT PN=1.4kW; UDC=600V M0=16Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",3016,"ΤΕΜ",1,"MC",1,"1FK70832AH711DG1"]
["1FK7084-2AC71-1DH2","SIMOTICS S Synchronous motor 1FK7-CT PN=3.1kW; UDC=600V M0=20Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) Smooth shaft, tolerance N With holding brake PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3791,"ΤΕΜ",1,"MC",1,"1FK70842AC711DH2"]
["1FK7084-2AC71-1QA2","SIMOTICS S synchronous motor 1FK7-CT PN=3.1 kW; UDC=600 V M0=20 Nm (100K); NN=2000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65 DE flange IP67",2820,"ΤΕΜ",1,"MC",1,"1FK70842AC711QA2"]
["1FK7084-2AF71-1QA1","SIMOTICS S synchronous motor 1FK7-CT PN=3.1kW; UDC=600V M0=20Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake, degree of protection IP65",2820,"ΤΕΜ",1,"MC",1,"1FK70842AF711QA1"]
["1FK7084-2AF74-1AG2","SIMOTICS S Synchronous motor 1FK7-CT PN=3.1kW; UDC=600V M0=20Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2988,"ΤΕΜ",1,"MC",1,"1FK70842AF741AG2"]
["1FK7084-3BC71-1QH2","SIMOTICS S synchronous motor 1FK7-HI PN=3.1kW; UDC=600V M0=20Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) Smooth shaft, tolerance N with holding brake, degree of protection IP65 DE Flange, IP67",3175,"ΤΕΜ",1,"MC",1,"1FK70843BC711QH2"]
["1FK7084-3BF74-1AB2","SIMOTICS S Synchronous motor 1FK7-HI PN=3.1kW; UDC=600V M0=20Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VP 2048 S/R WITH C- AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3534,"ΤΕΜ",1,"MC",1,"1FK70843BF741AB2"]
["1FK7085-4CC71-1RB0","SIMOTICS S Synchronous motor 1FK7-HD PN=3.1kW; UDC=600V M0=22Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3729,"ΤΕΜ",1,"MC",1,"1FK70854CC711RB0"]
["1FK7085-4CC74-1AB2","SIMOTICS S Synchronous motor 1FK7-HD PN=3.1kW; UDC=600V M0=22Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",3685,"ΤΕΜ",1,"MC",1,"1FK70854CC741AB2"]
["1FK7085-4CF74-1SA1","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=22Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2595,"ΤΕΜ",1,"MC",1,"1FK70854CF741SA1"]
["1FK7086-4CC71-1QH1","SIMOTICS S Synchronous motor 1FK7-HD PN=3.8kW; UDC=600V M0=28Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3762,"ΤΕΜ",1,"MC",1,"1FK70864CC711QH1"]
["1FK7086-4CC74-1SA2","SIMOTICS S Synchronous motor 1FK7-HD PN=3.8kW; UDC=600V M0=28Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",3030,"ΤΕΜ",1,"MC",1,"1FK70864CC741SA2"]
["1FK7086-4CF71-1UA0","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=28Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",3193,"ΤΕΜ",1,"MC",1,"1FK70864CF711UA0"]
["1FK7100-2AC71-1BB2","SIMOTICS S synchronous motor 1FK7-CT PN=3 kW; UDC=600V M0=18Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",3743,"ΤΕΜ",1,"MC",1,"1FK71002AC711BB2"]
["1FK7100-2AC74-1SG0","SIMOTICS S synchronous motor 1FK7-CT PN=3 kW; UDC=600V M0=18Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=4) smooth shaft, tolerance N without holding brake, type of protection IP64",2193,"ΤΕΜ",1,"MC",1,"1FK71002AC741SG0"]
["1FK7100-2AF71-1UG2","SIMOTICS S synchronous motor 1FK7-CT PN=3.8 kW; UDC=600 V M0=18 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake degree of protection IP65 DE flange IP67",2558,"ΤΕΜ",1,"MC",1,"1FK71002AF711UG2"]
["1FK7100-3BC71-1CH1","SIMOTICS S synchronous motor 1FK7-HI PN=3 kW; UDC=600V M0=18Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",4043,"ΤΕΜ",1,"MC",1,"1FK71003BC711CH1"]
["1FK7101-2AC71-1BH2","SIMOTICS S Synchronous motor 1FK7-CT PN=4.3kW; UDC=600V M0=27Nm (100K); NN=2000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with holding brake IP65 degree of protection DE flange IP67",3999,"ΤΕΜ",1,"MC",1,"1FK71012AC711BH2"]
["1FK7101-2AC71-1PA2","SIMOTICS S synchronous motor 1FK7-CT PN=4.3 kW; UDC=600 V M0=27 Nm (100K); NN=2000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake degree of protection IP65 DE flange IP67",3003,"ΤΕΜ",1,"MC",1,"1FK71012AC711PA2"]
["1FK7101-2AF71-1BG1","SIMOTICS S synchronous motor 1FK7-CT PN=4.9kW; UDC=600V M0=27Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) Smooth shaft, tolerance N without holding brake, degree of protection IP65",3549,"ΤΕΜ",1,"MC",1,"1FK71012AF711BG1"]
["1FK7101-2AF71-1UG2","SIMOTICS S synchronous motor 1FK7-CT PN=4.9 kW; UDC=600 V M0=27 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake degree of protection IP65 DE flange IP67",2909,"ΤΕΜ",1,"MC",1,"1FK71012AF711UG2"]
["1FK7101-3BC71-1RG2","SIMOTICS S synchronous motor 1FK7-HI PN=4.3kW; UDC=600V M0=27Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 20-bit + 12-bit multiturn with DRIVE-CLiQ interface (encoder AM20DQI) Smooth shaft, tolerance N without holding brake, degree of protection IP65 DE Flange, IP67",3416,"ΤΕΜ",1,"MC",1,"1FK71013BC711RG2"]
["1FK7103-2AC71-1CH1","SIMOTICS S Synchronous motor 1FK7-CT PN=5.2kW; UDC=600V M0=36Nm (100K); NN=2000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake IP65 degree of protection",4864,"ΤΕΜ",1,"MC",1,"1FK71032AC711CH1"]
["1FK7103-2AC71-1UA2","SIMOTICS S synchronous motor 1FK7-CT PN=5.2 kW; UDC=600 V M0=36 Nm (100K); NN=2000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake degree of protection IP65 DE flange IP67",3465,"ΤΕΜ",1,"MC",1,"1FK71032AC711UA2"]
["1FK7103-2AF71-1DH1","SIMOTICS S Synchronous motor 1FK7-CT PN=4.4kW; UDC=600V M0=36Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",4546,"ΤΕΜ",1,"MC",1,"1FK71032AF711DH1"]
["1FK7103-2AF74-1SB1","SIMOTICS S synchronous motor 1FK7-CT PN=4.4 kW; UDC=600V M0=36 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=4) shaft with feather key, tolerance N with holding brake degree of protection IP65",3651,"ΤΕΜ",1,"MC",1,"1FK71032AF741SB1"]
["1FK7103-3BF71-1BH0","SIMOTICS S synchronous motor 1FK7-HI PN=4.4 kW; UDC=600V M0=36 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",4340,"ΤΕΜ",1,"MC",1,"1FK71033BF711BH0"]
["1FK7103-3BF71-1QG0","SIMOTICS S synchronous motor 1FK7-HI PN=4.4 kW; UDC=600V M0=36 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",3362,"ΤΕΜ",1,"MC",1,"1FK71033BF711QG0"]
["1FK7105-2AC71-1DB1","SIMOTICS S Synchronous motor 1FK7-CT PN=7.7kW; UDC=600V M0=48Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",5801,"ΤΕΜ",1,"MC",1,"1FK71052AC711DB1"]
["1FK7105-2AF71-1FG1","SIMOTICS S Synchronous motor 1FK7-CT PN=8.2kW; UDC=600V M0=48Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",5660,"ΤΕΜ",1,"MC",1,"1FK71052AF711FG1"]
["1FK7105-2AF71-1QH0","SIMOTICS S Synchronous motor 1FK7-CT PN=8.2kW; UDC=600V M0=48Nm (100K); NN=3000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with holding brake IP64 degree of protection",4991,"ΤΕΜ",1,"MC",1,"1FK71052AF711QH0"]
["1FK7105-3BC71-1QB0","SIMOTICS S synchronous motor 1FK7-HI PN=7.7kW; UDC=600V M0=48Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake, degree of protection IP64",5057,"ΤΕΜ",1,"MC",1,"1FK71053BC711QB0"]
["1FL6034-2AF21-1AA1","SIMOTICS S-1FL6 Operating voltage 230 V 3AC Pn=0.4 kW; Nn=3000 rpm M0=1.27 Nm; MN=1.27 Nm Shaft height 30 mm Incremental encoder TTL 2500 incr./rev. with feather key Tolerance N without holding brake Degree of protection IP65 with sealing ring compatible with the converters SINAMICS V90",475,"ΤΕΜ",1,"MC",1,"1FL60342AF211AA1"]
["1FL6064-1AC61-2AA1","SIMOTICS S-1FL6-1FL6 Operating voltage 3AC 400 V Pn=1.5 kW; Nn=2000 rpm M0=8 Nm; MN=7.16 Nm Shaft height 65 mm, with angle plug; incremental encoder 2500 incr./rev. with feather key, tolerance N without holding brake Degree of protection IP65 with sealing ring compatible with the converters SINAMICS V70 & V90",863,"ΤΕΜ",1,"MC",1,"1FL60641AC612AA1"]
["1FL6094-1AC61-2LB1","SIMOTICS S-1FL6-1FL6 Operating voltage 3AC 400 V Pn=5 kW; Nn=2000 rpm M0=30 Nm; MN=23.9 Nm Shaft height 90 mm, with angle plug; absolute encoder 20-bits (12-bit multi-turn) with feather key, tolerance with holding brake Degree of protection IP65 with sealing ring compatible with the converters SINAMICS V70 & V90",3152,"ΤΕΜ",1,"MC",1,"1FL60941AC612LB1"]
["1FT7034-5AK70-1FG2","SIMOTICS S Synchronous motor 1FT7, M0=2Nm (100K) NN=6000rpm, PN=0.88kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",4500,"ΤΕΜ",1,"MC",1,"1FT70345AK701FG2"]
["1FT7036-5AK70-1DB1","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=6000rpm, PN=1.07kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4423,"ΤΕΜ",1,"MC",1,"1FT70365AK701DB1"]
["1FT7036-5AK71-1CA1","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=6000rpm, PN=1.07kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4478,"ΤΕΜ",1,"MC",1,"1FT70365AK711CA1"]
["1FT7042-5AF70-1CE3","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=3000rpm, PN=0.85kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",5509,"ΤΕΜ",1,"MC",1,"1FT70425AF701CE3"]
["1FT7042-5AF71-1DG0","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=3000rpm, PN=0.85kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",3670,"ΤΕΜ",1,"MC",1,"1FT70425AF711DG0"]
["1FT7042-5AK71-1BH0","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=6000rpm, PN=1.26kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",4332,"ΤΕΜ",1,"MC",1,"1FT70425AK711BH0"]
["1FT7042-5AK71-1DG1","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=6000rpm, PN=1.26kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",3775,"ΤΕΜ",1,"MC",1,"1FT70425AK711DG1"]
["1FT7044-5AF71-1BH5","SIMOTICS S Synchronous motor 1FT7, M0=5Nm (100K) NN=3000rpm, PN=1.35kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",5091,"ΤΕΜ",1,"MC",1,"1FT70445AF711BH5"]
["1FT7044-5AK70-1BG1","SIMOTICS S Synchronous motor 1FT7, M0=5Nm (100K) NN=6000rpm, PN=1.41kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4084,"ΤΕΜ",1,"MC",1,"1FT70445AK701BG1"]
["1FT7044-5AK71-1DG0","SIMOTICS S Synchronous motor 1FT7, M0=5Nm (100K) NN=6000rpm, PN=1.41kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",4066,"ΤΕΜ",1,"MC",1,"1FT70445AK711DG0"]
["1FT7044-5AK71-1FG3","SIMOTICS S Synchronous motor 1FT7, M0=5Nm (100K) NN=6000rpm, PN=1.41kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",5072,"ΤΕΜ",1,"MC",1,"1FT70445AK711FG3"]
["1FT7046-5AF71-1CA4","SIMOTICS S Synchronous motor 1FT7, M0=7Nm (100K) NN=3000rpm, PN=1.76kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",5424,"ΤΕΜ",1,"MC",1,"1FT70465AF711CA4"]
["1FT7046-5AH70-1DG0","SIMOTICS S Synchronous motor 1FT7, M0=7Nm (100K) NN=4500rpm, PN=1.32kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",4400,"ΤΕΜ",1,"MC",1,"1FT70465AH701DG0"]
["1FT7062-5AF71-1BA0","SIMOTICS S Synchronous motor 1FT7, M0=6Nm (100K) NN=3000rpm, PN=1.70kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",3921,"ΤΕΜ",1,"MC",1,"1FT70625AF711BA0"]
["1FT7062-5AF71-1CG2","SIMOTICS S Synchronous motor 1FT7, M0=6Nm (100K) NN=3000rpm, PN=1.70kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",4949,"ΤΕΜ",1,"MC",1,"1FT70625AF711CG2"]
["1FT7062-5AK71-1DA2","SIMOTICS S Synchronous motor 1FT7, M0=6Nm (100K) NN=6000rpm, PN=2.13kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",4201,"ΤΕΜ",1,"MC",1,"1FT70625AK711DA2"]
["1FT7062-5WK71-1CH1","SIMOTICS S Synchronous motor 1FT7, M0=10Nm (100K) NN=6000rpm, PN=5.80kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6436,"ΤΕΜ",1,"MC",1,"1FT70625WK711CH1"]
["1FT7064-5AF70-1DH2","SIMOTICS S Synchronous motor 1FT7, M0=9Nm (100K) NN=3000rpm, PN=2.39kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",5532,"ΤΕΜ",1,"MC",1,"1FT70645AF701DH2"]
["1FT7064-5AF71-1CA0","SIMOTICS S Synchronous motor 1FT7, M0=9Nm (100K) NN=3000rpm, PN=2.39kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5221,"ΤΕΜ",1,"MC",1,"1FT70645AF711CA0"]
["1FT7064-5AK71-1DA1","SIMOTICS S Synchronous motor 1FT7, M0=9Nm (100K) NN=6000rpm, PN=2.59kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4578,"ΤΕΜ",1,"MC",1,"1FT70645AK711DA1"]
["1FT7064-5WK71-1CG1","SIMOTICS S Synchronous motor 1FT7, M0=16Nm (100K) NN=6000rpm, PN=8.90kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6027,"ΤΕΜ",1,"MC",1,"1FT70645WK711CG1"]
["1FT7066-5AF70-1DA1","SIMOTICS S Synchronous motor 1FT7, M0=12Nm (100K) NN=3000rpm, PN=2.92kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4916,"ΤΕΜ",1,"MC",1,"1FT70665AF701DA1"]
["1FT7066-5AF70-1FB4","SIMOTICS S Synchronous motor 1FT7, M0=12Nm (100K) NN=3000rpm, PN=2.92kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE Absolute encoder 22-bit Multiturn with DRIVE-CLiQ interface (encoder AM22DQ) Rotatable connector SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",6790,"ΤΕΜ",1,"MC",1,"1FT70665AF701FB4"]
["1FT7066-5AH70-1CH0","SIMOTICS S Synchronous motor 1FT7, M0=12Nm (100K) NN=4500rpm, PN=2.55kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6427,"ΤΕΜ",1,"MC",1,"1FT70665AH701CH0"]
["1FT7066-5AH71-1FG0","SIMOTICS S Synchronous motor 1FT7, M0=12Nm (100K) NN=4500rpm, PN=2.55kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE Absolute encoder 22-bit Multiturn with DRIVE-CLiQ interface (encoder AM22DQ) Rotatable connector PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5647,"ΤΕΜ",1,"MC",1,"1FT70665AH711FG0"]
["1FT7067-7SF71-1CA1","SIMOTICS S Synchronous motor 1FT7, M0=17Nm (100K) NN=3000rpm, PN=4.40kW forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6756,"ΤΕΜ",1,"MC",1,"1FT70677SF711CA1"]
["1FT7068-5AF71-1DA0","SIMOTICS S Synchronous motor 1FT7, M0=15Nm (100K) NN=3000rpm, PN=3.42kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5149,"ΤΕΜ",1,"MC",1,"1FT70685AF711DA0"]
["1FT7068-5WF71-1DH1","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=3000rpm, PN=9.30kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6823,"ΤΕΜ",1,"MC",1,"1FT70685WF711DH1"]
["1FT7082-5AC70-1FG1","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=2000rpm, PN=2.39kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",5414,"ΤΕΜ",1,"MC",1,"1FT70825AC701FG1"]
["1FT7082-5AF70-1CH2","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=3000rpm, PN=3.24kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",6395,"ΤΕΜ",1,"MC",1,"1FT70825AF701CH2"]
["1FT7082-5AF71-1CB5","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=3000rpm, PN=3.24kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",6565,"ΤΕΜ",1,"MC",1,"1FT70825AF711CB5"]
["1FT7082-5AH70-1DG0","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=4500rpm, PN=3.77kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",4473,"ΤΕΜ",1,"MC",1,"1FT70825AH701DG0"]
["1FT7082-5AH71-1DG2","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=4500rpm, PN=3.77kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",4665,"ΤΕΜ",1,"MC",1,"1FT70825AH711DG2"]
["1FT7084-5AC70-1DE1","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=2000rpm, PN=3.54kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6552,"ΤΕΜ",1,"MC",1,"1FT70845AC701DE1"]
["1FT7084-5AC71-1KG2","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=2000rpm, PN=3.54kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) AND M17 CONNECTOR PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",5727,"ΤΕΜ",1,"MC",1,"1FT70845AC711KG2"]
["1FT7084-5AF71-1BD3","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=3000rpm, PN=4.55kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",5550,"ΤΕΜ",1,"MC",1,"1FT70845AF711BD3"]
["1FT7084-5AH70-1DG3","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=4500rpm, PN=4.82kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",5463,"ΤΕΜ",1,"MC",1,"1FT70845AH701DG3"]
["1FT7084-5AH71-1CA0","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=4500rpm, PN=4.82kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6043,"ΤΕΜ",1,"MC",1,"1FT70845AH711CA0"]
["1FT7084-5WC71-1DA0","SIMOTICS S Synchronous motor 1FT7, M0=35Nm (100K) NN=2000rpm, PN=7.33kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5995,"ΤΕΜ",1,"MC",1,"1FT70845WC711DA0"]
["1FT7084-5WF71-1BH1","SIMOTICS S Synchronous motor 1FT7, M0=35Nm (100K) NN=3000rpm, PN=11.00kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6994,"ΤΕΜ",1,"MC",1,"1FT70845WF711BH1"]
["1FT7085-7WH71-1CH1","SIMOTICS S Synchronous motor 1FT7, M0=43Nm (100K) NN=4500rpm, PN=15.60kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",8890,"ΤΕΜ",1,"MC",1,"1FT70857WH711CH1"]
["1FT7086-5AC70-1BG2","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=2000rpm, PN=4.71kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",6462,"ΤΕΜ",1,"MC",1,"1FT70865AC701BG2"]
["1FT7086-5AC71-1CH5","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=2000rpm, PN=4.71kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",8450,"ΤΕΜ",1,"MC",1,"1FT70865AC711CH5"]
["1FT7086-5AF70-1CH0","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=3000rpm, PN=5.65kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",8088,"ΤΕΜ",1,"MC",1,"1FT70865AF701CH0"]
["1FT7086-5AF71-1CB0","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=3000rpm, PN=5.65kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",8088,"ΤΕΜ",1,"MC",1,"1FT70865AF711CB0"]
["1FT7086-5AH70-1DK1","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=4500rpm, PN=4.71kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6637,"ΤΕΜ",1,"MC",1,"1FT70865AH701DK1"]
["1FT7086-5SF71-1BA1","SIMOTICS S Synchronous motor 1FT7, M0=36Nm (100K) NN=3000rpm, PN=9.10kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7076,"ΤΕΜ",1,"MC",1,"1FT70865SF711BA1"]
["1FT7086-5WC71-1CE3","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=2000rpm, PN=10.50kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",9129,"ΤΕΜ",1,"MC",1,"1FT70865WC711CE3"]
["1FT7086-5WH71-1KH2","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=4500rpm, PN=20.30kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) AND M17 CONNECTOR PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",8473,"ΤΕΜ",1,"MC",1,"1FT70865WH711KH2"]
["1FT7087-7SF71-1CL4","SIMOTICS S Synchronous motor 1FT7, M0=48Nm (100K) NN=3000rpm, PN=10.40kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",10106,"ΤΕΜ",1,"MC",1,"1FT70877SF711CL4"]
["1FT7087-7WH70-1CB0","SIMOTICS S Synchronous motor 1FT7, M0=61Nm (100K) NN=4500rpm, PN=21.70kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",9659,"ΤΕΜ",1,"MC",1,"1FT70877WH701CB0"]
["1FT7102-5AB70-1DG1","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=1500rpm, PN=4.08kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6125,"ΤΕΜ",1,"MC",1,"1FT71025AB701DG1"]
["1FT7102-5AC71-1BA0","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=2000rpm, PN=5.03kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5932,"ΤΕΜ",1,"MC",1,"1FT71025AC711BA0"]
["1FT7102-5AF70-1BB4","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=3000rpm, PN=6.28kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",7314,"ΤΕΜ",1,"MC",1,"1FT71025AF701BB4"]
["1FT7102-5AF71-1DG1","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=3000rpm, PN=6.28kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6125,"ΤΕΜ",1,"MC",1,"1FT71025AF711DG1"]
["1FT7102-5WF71-1DH0","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=3000rpm, PN=14.30kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",7827,"ΤΕΜ",1,"MC",1,"1FT71025WF711DH0"]
["1FT7105-5AB70-1CH0","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=1500rpm, PN=6.60kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",9543,"ΤΕΜ",1,"MC",1,"1FT71055AB701CH0"]
["1FT7105-5AB71-1CD4","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=1500rpm, PN=6.60kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",8886,"ΤΕΜ",1,"MC",1,"1FT71055AB711CD4"]
["1FT7105-5AC70-1BH3","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=2000rpm, PN=7.96kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",8876,"ΤΕΜ",1,"MC",1,"1FT71055AC701BH3"]
["1FT7105-5AF70-1CB1","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=3000rpm, PN=8.80kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9648,"ΤΕΜ",1,"MC",1,"1FT71055AF701CB1"]
["1FT7105-5AF70-1FH3","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=3000rpm, PN=8.80kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",9800,"ΤΕΜ",1,"MC",1,"1FT71055AF701FH3"]
["1FT7105-5AF71-1FB2","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=3000rpm, PN=8.80kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",9822,"ΤΕΜ",1,"MC",1,"1FT71055AF711FB2"]
["1FT7105-5SF70-1BG0","SIMOTICS S Synchronous motor 1FT7, M0=65Nm (100K) NN=3000rpm, PN=15.10kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",8300,"ΤΕΜ",1,"MC",1,"1FT71055SF701BG0"]
["1FT7105-5SF71-1BG1","SIMOTICS S Synchronous motor 1FT7, M0=65Nm (100K) NN=3000rpm, PN=15.10kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",8406,"ΤΕΜ",1,"MC",1,"1FT71055SF711BG1"]
["1FT7105-5WC70-1FA1","SIMOTICS S Synchronous motor 1FT7, M0=90Nm (100K) NN=2000rpm, PN=18.80kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9329,"ΤΕΜ",1,"MC",1,"1FT71055WC701FA1"]
["1FT7105-5WC71-1FG1","SIMOTICS S Synchronous motor 1FT7, M0=90Nm (100K) NN=2000rpm, PN=18.80kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9329,"ΤΕΜ",1,"MC",1,"1FT71055WC711FG1"]
["1FT7108-5AB71-1BA0","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=1500rpm, PN=9.58kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",9799,"ΤΕΜ",1,"MC",1,"1FT71085AB711BA0"]
["1FT7108-5AB71-1CB2","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=1500rpm, PN=9.58kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",11934,"ΤΕΜ",1,"MC",1,"1FT71085AB711CB2"]
["1FT7108-5AC70-1DH4","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=2000rpm, PN=10.50kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",11269,"ΤΕΜ",1,"MC",1,"1FT71085AC701DH4"]
["1FT7108-5AC71-1CL1","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=2000rpm, PN=10.50kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",12021,"ΤΕΜ",1,"MC",1,"1FT71085AC711CL1"]
["1FT7108-5AF70-1DG1","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=3000rpm, PN=6.28kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9992,"ΤΕΜ",1,"MC",1,"1FT71085AF701DG1"]
["1FT7108-5AF71-1CH2","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=3000rpm, PN=6.28kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",11934,"ΤΕΜ",1,"MC",1,"1FT71085AF711CH2"]
["1FT7108-5SF70-3BB0","SIMOTICS S Synchronous motor 1FT7, M0=91Nm (100K) NN=3000rpm, PN=18.80kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL NON-DRIVE END ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",11607,"ΤΕΜ",1,"MC",1,"1FT71085SF703BB0"]
["1FT7108-5SF71-8CH1","SIMOTICS S Synchronous motor 1FT7, M0=91Nm (100K) NN=3000rpm, PN=18.80kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) FOR CONNECT. OF TERMINAL BOXAND SIGNAL CONNECTOR, TERMINALBOX AXIAL DRIVE END ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",12548,"ΤΕΜ",1,"MC",1,"1FT71085SF718CH1"]
["1FT7108-5WC74-1MH0","SIMOTICS S Synchronous motor 1FT7, M0=125Nm (100K) NN=2000rpm, PN=26.20kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with Pt1000 temperature sensor POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",12059,"ΤΕΜ",1,"MC",1,"1FT71085WC741MH0"]
["1FT7108-5WF71-1CH0","SIMOTICS S Synchronous motor 1FT7, M0=125Nm (100K) NN=3000rpm, PN=34.20kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",12443,"ΤΕΜ",1,"MC",1,"1FT71085WF711CH0"]
["1FT7132-5AF71-1BH0","SIMOTICS S Synchronous motor 1FT7, M0=90Nm (100K) NN=3000rpm, PN=8.48kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",12831,"ΤΕΜ",1,"MC",1,"1FT71325AF711BH0"]
["1FT7132-5AF71-4CH2","SIMOTICS S Synchronous motor 1FT7, M0=90Nm (100K) NN=3000rpm, PN=8.48kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTION AXIAL DE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",13859,"ΤΕΜ",1,"MC",1,"1FT71325AF714CH2"]
["1FT7134-5AB71-1CL4","SIMOTICS S Synchronous motor 1FT7, M0=118Nm (100K) NN=1500rpm, PN=12.9kW naturally cooled; Power connector rotatable Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",15621,"ΤΕΜ",1,"MC",1,"1FT71345AB711CL4"]
["1FT7136-5AC71-4CB2","SIMOTICS S Synchronous motor 1FT7, M0=140Nm (100K) NN=2000rpm, PN=14.9kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTION AXIAL DE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",16376,"ΤΕΜ",1,"MC",1,"1FT71365AC714CB2"]
["1PH3107-1AG02-0LA0","Main motor for SINAMICS S120;3 Operating voltage 380 V 3AC Pn=11 kW; Nn=2000 rpm MN=53 Nm Axial height 100 mm IC22DQ Smooth shaft Forced ventilation, direction of air flow D IP54 compatible with the converters SI Vibration severity S Shaft end and flange precision Power and signal connection",4935,"ΤΕΜ",1,"MC",1,"1PH31071AG020LA0"]
["1PH8083-1DF00-2BB1","SIMOTICS M Compact induction motor 1500rpm, 2.8kW 18Nm, 7.5A, 346V 1750rpm, 3.3kW 18Nm, 7.5A, 398V 2000rpm, 3.7kW 18Nm, 7.6A, 447V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4979,"ΤΕΜ",1,"MC",1,"1PH80831DF002BB1"]
["1PH8083-1DG02-0BG1","SIMOTICS M Compact induction motor 2000rpm, 3.7kW 18Nm, 11.6A, 293V 2300rpm, 4.1kW 17Nm, 11.3A, 332V 2650rpm, 4.6 kW 17Nm, 11.2A, 376V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5145,"ΤΕΜ",1,"MC",1,"1PH80831DG020BG1"]
["1PH8083-1DM00-2DA1","SIMOTICS M Compact induction motor 3000rpm, 4.1kW 13Nm, 13.6A, 293V 3300RPM, 4.5kW 13Nm, 13.5A, 332V 3600RPM 4.9kW 13Nm, 14A, 376V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE SR/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5269,"ΤΕΜ",1,"MC",1,"1PH80831DM002DA1"]
["1PH8083-1ST22-0NE1","SIMOTICS M Compact induction motor 12000rpm 9.0kW 7.2Nm 24.0A 336V 13000RPM 9.8kW 7.2Nm 24.0A 367V 4 kHz pulse frequency water cooling Degree of protection IP65 Incremental encoder 19-bit Without commutation position (encoder IN19DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PREMIUM PERFORMANCE VIBRATION SEVERITY GRADE SPECIAL/B SHAFT AND FLANGE ACCURACY GR. SPECIAL POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9653,"ΤΕΜ",1,"MC",1,"1PH80831ST220NE1"]
["1PH8087-1DF12-1CA1","SIMOTICS M Compact induction motor 1500rpm, 3.7kW, 24Nm, 10A, 336V 1750rpm, 4.3kW, 23Nm, 10A, 396V 2000rpm, 4.9kW, 23Nm, 10A, 435V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5540,"ΤΕΜ",1,"MC",1,"1PH80871DF121CA1"]
["1PH8087-1DG02-0LE1","SIMOTICS M Compact induction motor 2000rpm, 4.9kW 23Nm, 14.1A, 320V 2300rpm, 5.4kW 22Nm, 13.7A, 353V 2650rpm, 6.0kW 22Nm, 13.6A, 390V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5925,"ΤΕΜ",1,"MC",1,"1PH80871DG020LE1"]
["1PH8087-1SG02-1LB1","SIMOTICS M Compact induction motor 2000rpm, 4.9kW 23Nm, 14.1A, 320V 2300rpm, 5.4kW 22Nm, 13.7A, 353V 2650rpm, 6.0kW 22Nm, 13.6A, 390V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 19-bit Without commutation position (encoder IN19DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",7394,"ΤΕΜ",1,"MC",1,"1PH80871SG021LB1"]
["1PH8101-1DF00-1BA1","SIMOTICS M Compact induction motor 1500rpm, 3.7kW 24Nm, 12.5A, 265V 2000rpm, 4.3kW 22Nm, 12.5A, 304V 2000rpm, 4.7kW 22Nm, 12.5A, 343V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5239,"ΤΕΜ",1,"MC",1,"1PH81011DF001BA1"]
["1PH8101-1SS02-1LA1","SIMOTICS M Compact induction motor Y2000RPM, 4.9kW 23Nm, 13.2A, 328V D5000RPM, 4.9kW 9Nm, 13.5A, 360V Y1500RPM, 3.7kW 24Nm, 13.2A, 253V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 19-bit Without commutation position (encoder IN19DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7481,"ΤΕΜ",1,"MC",1,"1PH81011SS021LA1"]
["1PH8103-1DD03-0BA1","SIMOTICS M Compact induction motor 1000rpm, 3.7kW 35Nm, 10.0A, 333V 1150rpm, 4.3kW 36Nm, 10.0A, 380 V 1350rpm, 4.7kW 33Nm, 9.7A, 423V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5830,"ΤΕΜ",1,"MC",1,"1PH81031DD030BA1"]
["1PH8103-1DF12-2BA1","SIMOTICS M Compact induction motor 1500rpm, 5.5 kW 35Nm, 13.1A, 368V 1750rpm, 6.3kW 34Nm, 13.5A, 412V 2000rpm, 7 kW 33Nm, 12.7A, 460 V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5569,"ΤΕΜ",1,"MC",1,"1PH81031DF122BA1"]
["1PH8103-1DG03-2GC1","SIMOTICS M Compact induction motor 2000rpm, 7.0 kW 31Nm, 17A, 345V 2300rpm, 7.5kW 33Nm, 17.5A, 400 V 2650rpm, 8.0kW 29Nm, 16A, 434V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5518,"ΤΕΜ",1,"MC",1,"1PH81031DG032GC1"]
["1PH8103-1DM22-0CE1","SIMOTICS M Compact induction motor 3000rpm, 10.6kW 34Nm, 30 A, 309V 3300RPM, 11.7kW 34Nm, 30 A, 340V 3600RPM 12.7kW 34Nm, 29.7A, 368V water cooling Degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6235,"ΤΕΜ",1,"MC",1,"1PH81031DM220CE1"]
["1PH8103-1FG00-1BA1","SIMOTICS M Compact induction motor 2000rpm, 7.0 kW 31Nm, 17A, 345V 2300rpm, 7.5kW 33Nm, 17.5A, 400 V 2650rpm, 8.0kW 29Nm, 16A, 434V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6351,"ΤΕΜ",1,"MC",1,"1PH81031FG001BA1"]
["1PH8103-1HM00-2FA2","SIMOTICS M Compact asynchronous motor 3000 rpm, 8.4 kW, 27 Nm, 25.7 A, 297 V 3300 rpm, 9.3 kW, 27 Nm, 25.7 A, 326 V 3600 rpm, 10 kW, 27 Nm, 25.4 A, 355 V Forced ventilation; Direction of air flow DE --> NDE; Degree of protection IP55 Incremental encoder HTL 1024 S/R (encoder HTL1024S/R) With temperature sensor Pt1000 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: INCREASED RADIAL FORCES, VIBRATION SEVERITY GRADE: R/A, SHAFT+FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4333,"ΤΕΜ",1,"MC",1,"1PH81031HM002FA2"]
["1PH8105-1DF00-2CA1","SIMOTICS M Compact induction motor 1500rpm, 7.0 kW 45Nm, 17.5A, 348V 1750rpm, 8.0kW 44Nm, 17.5A, 400 V 2000rpm, 9.0kW 43Nm, 17.0A, 453V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5777,"ΤΕΜ",1,"MC",1,"1PH81051DF002CA1"]
["1PH8105-1DF10-1CA1","SIMOTICS M Compact induction motor 1500rpm, 7kW, 45Nm, 17.5A, 348V 1750rpm, 8kW, 44Nm, 17.5A, 400 V 2000rpm, 9kW, 43Nm, 17A, 453V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5777,"ΤΕΜ",1,"MC",1,"1PH81051DF101CA1"]
["1PH8105-1FG20-0BA1","SIMOTICS M Compact induction motor 2000rpm, 13kW 62Nm, 34.5A, 326V 2300rpm, 15 kW 62Nm, 34A, 370V 2650rpm, 17kW 61Nm, 33.5A, 424V water cooling Degree of protection IP65 Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7135,"ΤΕΜ",1,"MC",1,"1PH81051FG200BA1"]
["1PH8107-1DD02-2BE1","SIMOTICS M Compact induction motor 1000rpm, 6.3kW 60Nm, 17.5A, 307V 1150rpm, 7.2kW 60Nm, 17.5A, 348V 1350rpm, 8.0kW 57Nm, 17A, 400 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5932,"ΤΕΜ",1,"MC",1,"1PH81071DD022BE1"]
["1PH8107-1DF00-0BA1","SIMOTICS M Compact induction motor 1500rpm, 9.0kW 57Nm, 23.5A, 330V 1750rpm, 10.0kW 55Nm, 22A, 380 V 2000rpm, 11 kW 53Nm, 21.5A, 428V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5719,"ΤΕΜ",1,"MC",1,"1PH81071DF000BA1"]
["1PH8107-1DF12-0BB1","SIMOTICS M Compact induction motor 1500rpm, 9kW 57Nm, 23.5A, 330V 1750rpm, 10 kW 55Nm, 22A, 380 V 2000rpm, 11 kW 53Nm, 21.5A, 428V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5932,"ΤΕΜ",1,"MC",1,"1PH81071DF120BB1"]
["1PH8107-1DF22-0DC1","SIMOTICS M Compact induction motor 1500rpm, 14kW 89Nm, 43.4A, 277V 1750rpm, 15.5kW 85Nm, 42A, 314V 2000rpm, 18kW 86Nm, 42.6A, 363V water cooling Degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: SR/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",7022,"ΤΕΜ",1,"MC",1,"1PH81071DF220DC1"]
["1PH8107-1DM00-1BA1","SIMOTICS M Compact induction motor 3000rpm, 12kW 38Nm, 38A, 294V 3300RPM, 13kW 38Nm, 38A, 326V 3600RPM 14kW 37Nm, 37.5A, 355V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5719,"ΤΕΜ",1,"MC",1,"1PH81071DM001BA1"]
["1PH8107-1DM02-0DA1","SIMOTICS M Compact induction motor 3000rpm, 12kW 38Nm, 38A, 294V 3300RPM, 13kW 38Nm, 38A, 326V 3600RPM 14kW 37Nm, 37.5A, 355V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: SR/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6222,"ΤΕΜ",1,"MC",1,"1PH81071DM020DA1"]
["1PH8107-1FD13-0BA1","SIMOTICS M Compact induction motor 1000rpm, 6.3kW 60Nm, 17.5A, 307V 1150rpm, 7.2kW 60Nm, 17.5A, 348V 1350rpm, 8kW 57Nm, 17A, 400 V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7188,"ΤΕΜ",1,"MC",1,"1PH81071FD130BA1"]
["1PH8107-1SG12-3MC1","SIMOTICS M Compact induction motor 2000rpm, 10.5kW 50Nm, 26 A, 355V 2300rpm, 12.5kW 50Nm, 26 A, 406V 2650rpm, 13kW 47Nm, 24A, 460 V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 19-bit Without commutation position (encoder IN19DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN HOLLOW-SHAFT BEARING: HIGH PERFORMANCE VIBRATION SEVERITY GRADE SPECIAL/B SHAFT AND FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",10203,"ΤΕΜ",1,"MC",1,"1PH81071SG123MC1"]
["1PH8131-1DF00-0DC1","SIMOTICS M Compact induction motor 1500rpm, 11kW, 70 Nm, 24A, 360V 1750rpm, 13kW, 71Nm, 24A, 416V 2000rpm, 15 kW, 72Nm, 24A, 460 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: SR/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",6182,"ΤΕΜ",1,"MC",1,"1PH81311DF000DC1"]
["1PH8131-1DF03-0CA1","SIMOTICS M Compact induction motor 1500rpm, 11kW, 70 Nm, 24A, 360V 1750rpm, 13kW, 71Nm, 24A, 416V 2000rpm, 15 kW, 72Nm, 24A, 460 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6698,"ΤΕΜ",1,"MC",1,"1PH81311DF030CA1"]
["1PH8131-1DG23-0BA1","SIMOTICS M Compact induction motor 2000rpm, 18kW, 86Nm, 40A, 352V 2300rpm, 20 kW, 83Nm, 39A, 400 V 2650rpm, 23kW, 83Nm, 39A, 458V water cooling Degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7325,"ΤΕΜ",1,"MC",1,"1PH81311DG230BA1"]
["1PH8131-2DF00-2CA1","SIMOTICS M Compact synchronous motor 1500rpm, 15.7kW 100 Nm, 29A, 388V 1750rpm, 18kW 98Nm, 29A, 415 V 2000rpm, 19.9kW 95Nm, 29A, 449V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",11946,"ΤΕΜ",1,"MC",1,"1PH81312DF002CA1"]
["1PH8133-1DB02-2GA1","SIMOTICS M Compact induction motor 400rpm 5.2kW 124Nm 15.5A 309V 500rpm 6.5kW 124Nm 15.5A 363V 600rpm 7.8kW 124Nm 15.5A 421V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5978,"ΤΕΜ",1,"MC",1,"1PH81331DB022GA1"]
["1PH8133-1DD00-0HB1","SIMOTICS M Compact induction motor 1000rpm, 12kW 115Nm, 30 A, 319V 1150rpm, 13.5kW 112Nm, 29A, 361V 1350rpm, 15 kW 106Nm, 28A, 417V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5931,"ΤΕΜ",1,"MC",1,"1PH81331DD000HB1"]
["1PH8133-1DF02-0BB1","SIMOTICS M Compact induction motor 1500rpm, 15 kW 96Nm, 34A, 342V 1750rpm, 17.5kW 96Nm, 34A, 392V 2000rpm, 20 kW 96Nm, 34A, 445V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",6290,"ΤΕΜ",1,"MC",1,"1PH81331DF020BB1"]
["1PH8133-1DF03-0CA1","SIMOTICS M Compact induction motor 1500rpm, 15 kW 96Nm, 34A, 342V 1750rpm, 17.5kW 96Nm, 34A, 392V 2000rpm, 20 kW 96Nm, 34A, 445V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6834,"ΤΕΜ",1,"MC",1,"1PH81331DF030CA1"]
["1PH8133-1DF20-0DC1","SIMOTICS M Compact induction motor 1500rpm, 17kW, 108Nm, 38A, 345V 1750rpm, 19.5kW, 106Nm, 38A, 40 2000rpm, 22.5kW, 107Nm, 38A, 45 water cooling Degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: SR/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",7200,"ΤΕΜ",1,"MC",1,"1PH81331DF200DC1"]
["1PH8133-1DG02-1BH1","SIMOTICS M Compact induction motor 2000rpm, 20 kW 96Nm, 45 A, 350 V 2300rpm, 22.5kW 93Nm, 44A, 400 V 2650rpm, 24 kW 86Nm, 41A, 456V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE D-END SIGNAL CONNECTION LEFT",6290,"ΤΕΜ",1,"MC",1,"1PH81331DG021BH1"]
["1PH8133-1FD12-2BE1","SIMOTICS M Compact induction motor 1000rpm, 12kW 115Nm, 30 A, 319V 1150rpm, 13.5kW 112Nm, 29A, 361V 1350rpm, 15 kW 106Nm, 28A, 417V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7285,"ΤΕΜ",1,"MC",1,"1PH81331FD122BE1"]
["1PH8133-1SF00-0LA1","SIMOTICS M Compact induction motor 1500rpm, 15 kW 96Nm, 34A, 342V 1750rpm, 17.5kW 96Nm, 34A, 392V 2000rpm, 20 kW 96Nm, 34A, 445V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 19-bit Without commutation position (encoder IN19DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8095,"ΤΕΜ",1,"MC",1,"1PH81331SF000LA1"]
["1PH8133-1UF22-1LA1","SIMOTICS M Compact induction motor 1500rpm, 17kW, 108Nm, 38A, 345V 1750rpm, 19.5kW, 106Nm, 38A, 40 2000rpm, 22.5kW, 107Nm, 38A, 45 water cooling Degree of protection IP65 Incremental encoder 20-bit Without commutation position (encoder IN20DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7994,"ΤΕΜ",1,"MC",1,"1PH81331UF221LA1"]
["1PH8133-2FL02-0BE1","SIMOTICS M Compact synchronous motor 2500rpm, 31.7kW 121Nm, 55A, 371V 2800rpm, 35.2kW 120Nm, 54A, 415 V 3000rpm, 37.4kW 119Nm, 54A, 449V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",13521,"ΤΕΜ",1,"MC",1,"1PH81332FL020BE1"]
["1PH8135-1DF00-1LA1","SIMOTICS M Compact induction motor 1500rpm, 18.5 kW 118Nm, 43A, 330V 1750rpm, 21.5kW 117Nm, 43A, 383V 2000rpm, 24 kW 115Nm, 43A, 434V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7083,"ΤΕΜ",1,"MC",1,"1PH81351DF001LA1"]
["1PH8135-1DF03-1BA1","SIMOTICS M Compact induction motor 1500rpm, 18.5 kW 118Nm, 43A, 330V 1750rpm, 21.5kW 117Nm, 43A, 383V 2000rpm, 24 kW 115Nm, 43A, 434V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7078,"ΤΕΜ",1,"MC",1,"1PH81351DF031BA1"]
["1PH8135-1DG20-0MA1","SIMOTICS M Compact induction motor 2000rpm, 29kW, 138Nm, 64A, 348V 2300rpm, 31kW, 129Nm, 61A, 397V 2650rpm, 32 kW, 115Nm, 58A, 448V water cooling Degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: HIGH PERFORMANCE VIBRATION SEVERITY GRADE SPECIAL/B SHAFT AND FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8859,"ΤΕΜ",1,"MC",1,"1PH81351DG200MA1"]
["1PH8135-1SG22-3LH1","SIMOTICS M Compact induction motor 2000rpm, 29kW, 138Nm, 64A, 348V 2300rpm, 31kW, 129Nm, 61A, 397V 2650rpm, 32 kW, 115Nm, 58A, 448V water cooling Degree of protection IP65 Incremental encoder 19-bit Without commutation position (encoder IN19DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN HOLLOW-SHAFT BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE D-END SIGNAL CONNECTION LEFT",11595,"ΤΕΜ",1,"MC",1,"1PH81351SG223LH1"]
["1PH8135-2DG23-0QA1","SIMOTICS M Compact synchronous motor 2000rpm, 39kW 186Nm, 81A, 346V 2300rpm, 44.3kW 184Nm, 80 A, 395V 2300rpm, 44.3kW 184Nm, 80 A, 395V water cooling Degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: ADVANCED LIFETIME VIBRATION SEVERITY S/A SHAFT A. FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",13752,"ΤΕΜ",1,"MC",1,"1PH81352DG230QA1"]
["1PH8137-1DD00-2BB1","SIMOTICS M Compact induction motor 1000rpm, 17kW 162Nm, 43A, 307V 1150rpm, 19.5kW 162Nm, 43A, 350 V 1350rpm, 22 kW 156Nm, 42A, 404V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",6787,"ΤΕΜ",1,"MC",1,"1PH81371DD002BB1"]
["1PH8137-1DD03-2GC1","SIMOTICS M Compact induction motor 1000rpm, 17kW 162Nm, 43A, 307V 1150rpm, 19.5kW 162Nm, 43A, 350 V 1350rpm, 22 kW 156Nm, 42A, 404V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",7068,"ΤΕΜ",1,"MC",1,"1PH81371DD032GC1"]
["1PH8137-1DF00-1DB1","SIMOTICS M Compact induction motor 1500rpm, 22kW, 140 Nm, 56A, 308V 1750rpm, 25kW, 136Nm, 56A, 352V 2000rpm, 28kW, 134Nm, 55A, 401V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: SR/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",7077,"ΤΕΜ",1,"MC",1,"1PH81371DF001DB1"]
["1PH8137-1DF13-1BB1","SIMOTICS M Compact induction motor 1500rpm, 22kW, 140 Nm, 56A, 308V 1750rpm, 25kW, 136Nm, 56A, 353V 2000rpm, 28kW, 134Nm, 55A, 401V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",7379,"ΤΕΜ",1,"MC",1,"1PH81371DF131BB1"]
["1PH8137-1DF23-1CE1","SIMOTICS M Compact induction motor 1500rpm, 27kW 172Nm, 67A, 315V 1750rpm, 31.5kW 172Nm, 67A, 365V 2000rpm, 36 kW 172Nm, 67A, 415 V water cooling Degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8912,"ΤΕΜ",1,"MC",1,"1PH81371DF231CE1"]
["1PH8137-1FD02-0GA1","SIMOTICS M Compact induction motor 1000rpm, 17kW 162Nm, 43A, 307V 1150rpm, 19.5kW 162Nm, 43A, 350 V 1350rpm, 22 kW 156Nm, 42A, 404V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7731,"ΤΕΜ",1,"MC",1,"1PH81371FD020GA1"]
["1PH8137-1FF00-0BA1","SIMOTICS M Compact induction motor 1500rpm, 22kW, 140 Nm, 56A, 308V 1750rpm, 25kW, 136Nm, 56A, 352V 2000rpm, 28kW, 134Nm, 55A, 401V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7782,"ΤΕΜ",1,"MC",1,"1PH81371FF000BA1"]
["1PH8137-1SG00-1LA1","SIMOTICS M Compact induction motor 2000rpm, 28kW, 134Nm, 60A, 350 V 2300rpm, 29kW, 120Nm, 56A, 400 V 2650rpm, 30 kW, 108Nm, 52A, 460 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 19-bit Without commutation position (encoder IN19DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8854,"ΤΕΜ",1,"MC",1,"1PH81371SG001LA1"]
["1PH8137-1UG00-0MA1","SIMOTICS M Compact induction motor 2000rpm, 28kW, 134Nm, 60A, 350 V 2300rpm, 29kW, 120Nm, 56A, 400 V 2650rpm, 30 kW, 108Nm, 52A, 460 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 20-bit Without commutation position (encoder IN20DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: HIGH PERFORMANCE VIBRATION SEVERITY GRADE SPECIAL/B SHAFT AND FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8095,"ΤΕΜ",1,"MC",1,"1PH81371UG000MA1"]
["1PH8137-2DL02-1BA1","SIMOTICS M Compact synchronous motor 2500rpm, 48.4kW 185Nm, 83A, 371V 2800rpm, 53.4kW 182Nm, 82A, 415 V 3000rpm, 56.9kW 181Nm, 81A, 449V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",14195,"ΤΕΜ",1,"MC",1,"1PH81372DL021BA1"]
["1PH8138-1DF22-1CA1","SIMOTICS M Compact induction motor 1500rpm, 30 kW, 191Nm, 80 A, 289V 1750rpm, 33 kW, 180Nm, 77A, 332V 2000rpm, 37kW, 177Nm, 76A, 380 V water cooling Degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8936,"ΤΕΜ",1,"MC",1,"1PH81381DF221CA1"]
["1PH8163-1CB03-0LA2","SIMOTICS M Compact asynchronous motor 400 rpm, 9.5 kW, 227 Nm, 30 A, 260 V 500 rpm, 12 kW, 229 Nm, 30 A, 325 V 600 rpm, 14.5 kW, 231 Nm, 30 A, 370 V Forced ventilation; Direction of air flow DE --> NDE; Degree of protection IP55 INCREMENTAL ENCODER SIN/COS 1VPP 256 S/R (ENCODER IN256S/R) with TEMPERAT. SENSOR PT1000 Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9955,"ΤΕΜ",1,"MC",1,"1PH81631CB030LA2"]
["1PH8163-1DD03-0LC1","SIMOTICS M Compact induction motor 1000rpm, 22kW, 210Nm, 55A, 300V 1150rpm, 25kW, 208Nm, 55A, 343V 1350rpm, 28kW, 198Nm, 52A, 400 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",9244,"ΤΕΜ",1,"MC",1,"1PH81631DD030LC1"]
["1PH8163-1DF00-2DA1","SIMOTICS M Compact induction motor 1500rpm, 30 kW, 191Nm, 71A, 319V 1750rpm, 34kW, 186Nm, 70A, 366V 2000rpm, 37kW, 177Nm, 68A, 416V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE SR/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8341,"ΤΕΜ",1,"MC",1,"1PH81631DF002DA1"]
["1PH8163-1DF10-2BB1","SIMOTICS M Compact induction motor 1500rpm, 30 kW, 191Nm, 71A, 319V 1750rpm, 34kW, 186Nm, 70A, 366V 2000rpm, 37kW, 177Nm, 68A, 416V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",8027,"ΤΕΜ",1,"MC",1,"1PH81631DF102BB1"]
["1PH8163-1DG00-0CA1","SIMOTICS M Compact induction motor 2000rpm, 36kW, 172Nm, 83A, 324V 2300rpm, 38 kW, 158Nm, 78A, 370V 2650rpm, 40kW, 144Nm, 76A, 390V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8027,"ΤΕΜ",1,"MC",1,"1PH81631DG000CA1"]
["1PH8163-1FD00-1BA1","SIMOTICS M Compact induction motor 1000rpm, 22kW, 210Nm, 55A, 300V 1150rpm, 25kW, 208Nm, 55A, 343V 1350rpm, 28kW, 198Nm, 52A, 400 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9022,"ΤΕΜ",1,"MC",1,"1PH81631FD001BA1"]
["1PH8163-1UD00-0LA1","SIMOTICS M Compact induction motor 1000rpm, 22kW, 210Nm, 55A, 300V 1150rpm, 25kW, 208Nm, 55A, 343V 1350rpm, 28kW, 198Nm, 52A, 400 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 20-bit Without commutation position (encoder IN20DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8759,"ΤΕΜ",1,"MC",1,"1PH81631UD000LA1"]
["1PH8165-1DD00-0HA1","SIMOTICS M Compact induction motor 1000rpm, 28kW, 267Nm, 71A, 292V 1150rpm, 31kW, 257Nm, 69A, 333V 1350rpm, 34kW, 241Nm, 66A, 387V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8320,"ΤΕΜ",1,"MC",1,"1PH81651DD000HA1"]
["1PH8165-1DD10-2DA1","SIMOTICS M Compact induction motor 1000rpm, 28kW, 267Nm, 71A, 292V 1150rpm, 31kW, 257Nm, 69A, 333V 1350rpm, 34kW, 241Nm, 66A, 387V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE SR/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8945,"ΤΕΜ",1,"MC",1,"1PH81651DD102DA1"]
["1PH8165-1DF03-0CA1","SIMOTICS M Compact induction motor 1500rpm, 37kW, 236Nm, 78A, 350 V 1750rpm, 41kW, 224Nm, 76A, 400 V 2000rpm, 45kW, 215Nm, 75 A, 440 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9342,"ΤΕΜ",1,"MC",1,"1PH81651DF030CA1"]
["1PH8165-1DF10-2BA1","SIMOTICS M Compact induction motor 1500rpm, 37kW, 236Nm, 78A, 350 V 1750rpm, 41kW, 224Nm, 76A, 400 V 2000rpm, 45kW, 215Nm, 75 A, 440 V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8631,"ΤΕΜ",1,"MC",1,"1PH81651DF102BA1"]
["1PH8165-1DG03-2BC1","SIMOTICS M Compact induction motor 2000rpm, 41kW, 196Nm, 88A, 350 V 2300rpm, 44 kW, 183Nm, 85A, 394V 2650rpm, 50 kW, 180Nm, 85A, 440 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",9342,"ΤΕΜ",1,"MC",1,"1PH81651DG032BC1"]
["1PH8165-1DG13-1GA1","SIMOTICS M Compact induction motor 2000rpm, 41kW, 196Nm, 88A, 350 V 2300rpm, 44 kW, 183Nm, 85A, 394V 2650rpm, 50 kW, 180Nm, 85A, 440 V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9031,"ΤΕΜ",1,"MC",1,"1PH81651DG131GA1"]
["1PH8165-1FF03-1BA1","SIMOTICS M Compact induction motor 1500rpm, 37kW, 236Nm, 78A, 350 V 1750rpm, 41kW, 224Nm, 76A, 400 V 2000rpm, 45kW, 215Nm, 75 A, 440 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",10337,"ΤΕΜ",1,"MC",1,"1PH81651FF031BA1"]
["1PH8165-2DF02-2BA1","SIMOTICS M Compact synchronous motor 1500rpm, 61kW 390Nm, 119A, 340V 1750rpm, 69kW 375Nm, 115A, 395V 2000rpm, 74kW 355Nm, 110 A, 445V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",17187,"ΤΕΜ",1,"MC",1,"1PH81652DF022BA1"]
["1PH8166-1FG23-2LC1","SIMOTICS M Compact induction motor 2000rpm, 64kW 306Nm, 125 A, 376V 2300rpm, 72kW 299Nm, 124A, 420V 2650rpm, 83kW 299Nm, 125 A, 460 V water cooling Degree of protection IP65 Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",14606,"ΤΕΜ",1,"MC",1,"1PH81661FG232LC1"]
["1PH8168-2DL23-2CA1","SIMOTICS M Compact synchronous motor 2500rpm, 119kW 455Nm, 225 A, 355V 2800rpm, 123kW 420Nm, 210A, 395V 3000rpm, 125kW 385Nm, 197A, 420V water cooling Degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",20254,"ΤΕΜ",1,"MC",1,"1PH81682DL232CA1"]
["1PH8184-1DL20-0BA1","SIMOTICS M Compact induction motor 2500rpm, 95kW 363Nm, 196A, 340V 2900rpm, 102kW 336Nm, 185A, 395V 3400rpm, 100 kW 281Nm, 158A, 460 V water cooling Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IMB6, IMB7, IMB8, IMV6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD VIBRATION SEVERITY GRADE R/A; SHAFT A.FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",15100,"ΤΕΜ",1,"MC",1,"1PH81841DL200BA1"]
["1PH8186-1DF03-0LC1","SIMOTICS M Compact induction motor 1500rpm, 74kW 471Nm, 166A, 330V 1750rpm, 85kW 464Nm, 164A, 385 V 2000rpm, 94kW 449Nm, 160 A, 445V forced ventilation Direction of air flow DE-->NDE Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 with flange A450 (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE VIBRATION SEVERITY GRADE SR/B SHAFT A. FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION RIGHT",23067,"ΤΕΜ",1,"MC",1,"1PH81861DF030LC1"]
["1PH8226-1DC05-0BA1","SIMOTICS M Compact induction motor 700 rpm, 68kW, 928Nm, 162A, 310V 800rpm, 73kW, 872Nm, 154A, 350 V 1000rpm, 92kW, 879Nm, 15 A, 440 V forced ventilation Direction of air flow DE-->NDE Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM V15 WITH FLANGE A550 PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD VIBRATION SEVERITY GRADE R/A; SHAFT A.FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",25293,"ΤΕΜ",1,"MC",1,"1PH82261DC050BA1"]
["6AU1810-1HA24-1XE0","SINAMICS ENGINEERING SYSTEM SINAMICS DCC V2.4 SP1 UPGRADE LICENSE DCC FOR SINAMICS OPTION TO STARTER V4.5 SP1 DELIVERY ON DATA CARRIER DVD INCL: FLOATING LICENSE",327,"ΤΕΜ",1,"MC",1,"6AU18101HA241XE0"]
["6FX2001-2MC04","INCREM. ENCODER 6FX2001-2MC04 WITH RS 422 (TTL), 2048 P/R, CLAMP FLANGE SHAFT 10MM OPERATING VOLTAGE 5 V, UNIVERSAL CABLE OUTGOING AXIAL / RADIAL CABLE 1M WITH CONNECTOR",396,"ΤΕΜ",1,"MC",1,"6FX20012MC04"]
["6FX2001-3GB00","INCREM. ENCODER 6FX2001-3GB00 WITH 1-V-SINUS 1000 P/R, SYNCHRON. FLANGE, 6 MM SHAFT, VOLTAGE 5 V AXIAL FLANGE CONNECTOR",396,"ΤΕΜ",1,"MC",1,"6FX20013GB00"]
["6FX2001-5FN13","ABS. VALUE ENCODER SINGLETURN 6FX2001-5FN13 13 BIT WITH PROFINET OPERATE VOLTAGE 10-30V SYNCHROFLANGE / SHAFT 6MM CONNECTOR M12 RADIAL",1208,"ΤΕΜ",1,"MC",1,"6FX20015FN13"]
["6FX2002-1DC00-1AJ0","Signal cable pre-assembled type: 6FX2002-1DC00 (SINAMICS Drive CLiQ) Connector IP20/IP20, without 24 V Length (m)= 0 + 0 + 8 + 0",167,"ΤΕΜ",1,"MC",1,"6FX20021DC001AJ0"]
["6FX2002-1DC00-1DG7","Signal cable pre-assembled type: 6FX2002-1DC00 (SINAMICS Drive CLiQ) Connector IP20/IP20, without 24 V Length (m)= 0 + 30 + 6 + 0,7",385,"ΤΕΜ",1,"MC",1,"6FX20021DC001DG7"]
["6FX2003-0FA00","DU box connector 4-pole type: 6FX2003-0FA00 (for device connection at cable distributor) Pack=10 connector enclosures and 40 contacts",62.9,"PAK",1,"MC",1,"6FX20030FA00"]
["6FX3002-2DB10-1BF0","Signal cable pre-assembled 6FX3002-2DB10 for ABS. encoder in S-1FL6 HI 3x 2x 0.22+2x2X0.25 MOTION-CONNECT 300 UL/CSA Dmax=7.8 mm Length (m)=15 m",211,"ΤΕΜ",1,"MC",1,"6FX30022DB101BF0"]
["6FX5002-2AD04-1BA5","signal cable, pre-assembled Extension (611D/MCU to encoder EnDat) 3x 2x 0.14+4x 0.14+2x0.5 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm TYPE: 6FX5002-2AD04 LENGTH (M) = 0 + 10 + 0 + 0,5",223,"ΤΕΜ",1,"MC",1,"6FX50022AD041BA5"]
["6FX5002-2AH11-1HA0","Signal cable pre-assembled type: 6FX5002-2AH11 (basis 6FX5002-2AH00-....) with integrated temperature cores UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm Length (m)= 0 + 70 + 0 + 0",768,"ΤΕΜ",1,"MC",1,"6FX50022AH111HA0"]
["6FX5002-2CA31-1AD7","signal cable pre-assembled (encoder voltage signal) 3x 2x 0.14+4x 0.14+2x0.5+4x 0.23 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.9 mm TYPE: 6FX5002-2CA31 LENGTH (M) = 0 + 0 + 3 + 0,7",153,"ΤΕΜ",1,"MC",1,"6FX50022CA311AD7"]
["6FX5002-2CF02-1BJ0","Signal cable pre-assembled (resolver in motor) 3x 2x 0.14+4x 0.14+2x0.5 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm Length (m)= TYPE: 6FX5002-2CF02 LENGTH (M) = 0 + 10 + 8 + 0",248,"ΤΕΜ",1,"MC",1,"6FX50022CF021BJ0"]
["6FX5002-2CF02-1DF0","Signal cable pre-assembled (resolver in motor) 3x 2x 0.14+4x 0.14+2x0.5 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm Length (m)= TYPE: 6FX5002-2CF02 LENGTH (M) = 0 + 30 + 5 + 0",361,"ΤΕΜ",1,"MC",1,"6FX50022CF021DF0"]
["6FX5002-2CQ31-1AB0","signal cable pre-assembled (encoder voltage signal) 3x 2x 0.14+4x 0.14+2x0.5+4x 0.23 C SPEED-CONNECT Connector UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.9 mm TYPE: 6FX5002-2CQ31 LENGTH (M) = + 0 + 0 + 1 + 0",128,"ΤΕΜ",1,"MC",1,"6FX50022CQ311AB0"]
["6FX5002-2DC10-1AF6","Signal cable pre-assembled type: 6FX5002-2DC10 (SINAMICS Drive CLiQ) connector IP20/IP67, with 24 V MOTION-CONNECT 500 Length (m)= 0 + 0 + 5 + 0,6",157,"ΤΕΜ",1,"MC",1,"6FX50022DC101AF6"]
["6FX5002-2DC10-1CB4","Signal cable pre-assembled type: 6FX5002-2DC10 (SINAMICS Drive CLiQ) connector IP20/IP67, with 24 V MOTION-CONNECT 500 Length (m)= 0 + 20 + 1 + 0,4",272,"ΤΕΜ",1,"MC",1,"6FX50022DC101CB4"]
["6FX5002-2DC20-1AA6","Signal cable pre-assembled type: 6FX5002-2DC20 (SINAMICS Drive CLiQ) connector IP67/IP67, with 24 V MOTION-CONNECT 500 Length (m)= 0 + 0 + 0 + 0,6",139,"ΤΕΜ",1,"MC",1,"6FX50022DC201AA6"]
["6FX5002-2DC30-2AA0","DRIVE-CLiQ cable Type: 6FX8002-2DC30 Pre-assembled for direct measuring systems with 24 V Connector RJ45, IP20 and Mating connector M12, IP67 MOTION-CONNECT 500 UL/CSA, DESINA Dmax=7.1 mm length (m)=100",922,"ΤΕΜ",1,"MC",1,"6FX50022DC302AA0"]
["6FX5002-2DC46-1FF0","Signal cable pre-assembled Type: 6FX5002-2DC46 DRIVE-CLiQ with 24 V M12 female/ M17 male speed-connect-ready MOTION-CONNECT 500 Dmax=7.1 mm length (m)=55",635,"ΤΕΜ",1,"MC",1,"6FX50022DC461FF0"]
["6FX5002-2DC46-1JF0","Signal cable pre-assembled Type: 6FX5002-2DC46 DRIVE-CLiQ with 24 V M12 female/ M17 male speed-connect-ready MOTION-CONNECT 500 Dmax=7.1 mm length (m)=85",904,"ΤΕΜ",1,"MC",1,"6FX50022DC461JF0"]
["6FX5002-2EQ14-1AJ0","signal cable, pre-assembled Extension (absolute encoder in motor) 3x 2x 0.14+4x 0.14+2x0.5+4x 0.22 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.9 mm TYPE: 6FX5002-2EQ14 LENGTH (M) = 0 + 0 + 8 + 0",222,"ΤΕΜ",1,"MC",1,"6FX50022EQ141AJ0"]
["6FX5002-5CG01-1CA0","Power cable pre-assembled type: 6FX5002-5CG01 4x 1.5 C, Connector Sz. 1 (SINAMICS AC Drive) UL/CSA, DESINA MOTION-CONNECT 500 Dmax=8.4 mm 0 + 20 + 0 + 0",221,"ΤΕΜ",1,"MC",1,"6FX50025CG011CA0"]
["6FX5002-5CG10-1AB5","Power cable pre-assembled 4x 1.5 C SPEED-CONNECT connector Sz. 1 (SINAMICS AC Drive) UL/CSA DESINA MOTION-CONNECT 500 Dmax=8.4 mm TYPE: 6FX5002-5CG10 LENGTH (M) = + 0 + 0 + 1 + 0,5",138,"ΤΕΜ",1,"MC",1,"6FX50025CG101AB5"]
["6FX5002-5CG22-1CG0","Power cable pre-assembled 4x 1.5 C Speed connect connector Sz. 1.5 (SINAMICS AC Drive) UL/CSA DESINA MOTION-CONNECT 500 Dmax=8.4 mm TYPE: 6FX5002-5CG22 LENGTH (M) = + 0 + 20 + 6 + 0",402,"ΤΕΜ",1,"MC",1,"6FX50025CG221CG0"]
["6FX5002-5CG41-1FA0","Power cable pre-assembled type: 6FX5002-5CG41 4x 4 C connector Sz. 1.5 (SINAMICS AC Drive) UL/CSA, DESINA MOTION-CONNECT 500 Dmax=11.4 mm 0 + 50 + 0 + 0",656,"ΤΕΜ",1,"MC",1,"6FX50025CG411FA0"]
["6FX5002-5CN06-1FF0","Power cable pre-assembled TYPE 6FX5002-5CN06 4X1,5 C, SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX=8.4 MM LENGTH (M) = + 0 + 50 + 5 + 0",422,"ΤΕΜ",1,"MC",1,"6FX50025CN061FF0"]
["6FX5002-5CR73-1CF0","Power cable pre-assembled type: 6FX5002-5CR73 4x 35 C, M50 screw connection for SINAMICS S120 Power Module MOTION-CONNECT 500 UL/CSA, DESINA Dmax=31.5 mm, Length (m)= 0 + 20 + 5 + 0",1586,"ΤΕΜ",1,"MC",1,"6FX50025CR731CF0"]
["6FX5002-5CS14-1BE0","Power cable pre-assembled type: 6FX5002-5CS14 (1FT/1FK/1PH for SINAMICS) 4x 10 C, Connector size 3 Ring cable lug UL/CSA, DESINA MOTION-CONNECT 500 Dmax=20 mm; Length (m)= 0 + 10 + 4 + 0",790,"ΤΕΜ",1,"MC",1,"6FX50025CS141BE0"]
["6FX5002-5CW12-1AD0","Power cable pre-assembled TYPE 6FX5002-5CW12 4X2,5 C, MOTOR SIDE WITH EXPOSED CORE ENDS FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX=10 MM LENGTH (M) = + 0 + 0 + 3 + 0",171,"ΤΕΜ",1,"MC",1,"6FX50025CW121AD0"]
["6FX5002-5DG01-1BE0","Power cable pre-assembled type: 6FX5002-5DG01 4x 1.5+(2x1.5) C, Connector Sz. 1 (SINAMICS AC Drive) UL/CSA, DESINA MOTION-CONNECT 500 Dmax=10.8 mm 0 + 10 + 4 + 0",260,"ΤΕΜ",1,"MC",1,"6FX50025DG011BE0"]
["6FX5002-5DG10-1AC0","Power cable pre-assembled 4x 1.5+(2x1.5) C SPEED-CONNECT connector Sz. 1 (SINAMICS AC Drive) UL/CSA DESINA MOTION-CONNECT 500 Dmax=10.8 mm TYPE: 6FX5002-5DG10 LENGTH (M) = + 0 + 0 + 2 + 0",164,"ΤΕΜ",1,"MC",1,"6FX50025DG101AC0"]
["6FX5002-5DG12-2GA0","Power cable pre-assembled 4x 2.5+(2x1.5) C C SPEED-CONNECT Sz. 1 for SINAMICS Power Module MOTION-CONNECT 500 UL/CSA DESINA Dmax=12.4 mm TYPE: 6FX5002-5DG12 LENGTH (M) = + 100 + 60 + 0 + 0",1729,"ΤΕΜ",1,"MC",1,"6FX50025DG122GA0"]
["6FX5002-5DG52-1BH0","Power cable pre-assembled 4x 6+(2x1.5) C Speed connect connector Sz. 1.5 (SINAMICS AC Drive) UL/CSA DESINA MOTION-CONNECT 500 Dmax=16.1 mm TYPE: 6FX5002-5DG52 LENGTH (M) = + 0 + 10 + 7 + 0",503,"ΤΕΜ",1,"MC",1,"6FX50025DG521BH0"]
["6FX5002-5DN36-1BF0","Power cable pre-assembled TYPE 6FX5002-5DN36 4X2.5 , (2X1.5)C C CONNECTOR SPEED-CONNECT SIZE 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX=12.4 MM LENGTH (M) = + 0 + 10 + 5 + 0",395,"ΤΕΜ",1,"MC",1,"6FX50025DN361BF0"]
["6FX5002-5DS06-1BF0","Power cable pre-assembled TYPE 6FX5002-5DS06 4X1.5, (2X1.5)C C CONNECTOR FULL THREAD SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX = 10.8 MM LENGTH (M) = + 0 + 10 + 5 + 0",314,"ΤΕΜ",1,"MC",1,"6FX50025DS061BF0"]
["6FX5002-5MN05-1AA3","power cable, pre-assembled, Extension 4x 1.5+(2x1.5) C C SPEED-CONNECT Sz. 0.5 MOTION-CONNECT 500 UL/CSA, DESINA Dmax=10.8 mm TYPE: 6FX5002-5MN05 LENGTH (M) = 0 + 0 + 0 + 0,3",209,"ΤΕΜ",1,"MC",1,"6FX50025MN051AA3"]
["6FX5008-1BA41-6AA0","Power cable sold by the meter type: 6FX5008-1BA41 4x 6.0+2x 1.5 C UL/CSA, DESINA MOTION-CONNECT 500 Type of delivery: Disposable drum Dmax=16.1 mm, Length (m)=500",9676,"ΤΕΜ",1,"MC",1,"6FX50081BA416AA0"]
["6FX5008-1BB21-3AA0","Power cable sold by the meter type: 6FX5008-1BB21 4x 2.5 C UL/CSA, DESINA MOTION-CONNECT 500 Type of delivery: Disposable drum Dmax=10 mm, Length (m)=200",1625,"ΤΕΜ",1,"MC",1,"6FX50081BB213AA0"]
["6FX5008-1BB25-2AA0","Power cable sold by the meter type: 6FX5008-1BB25 4x 25 C UL/CSA, DESINA MOTION-CONNECT 500 Type of delivery: up to 19 m ring from 20 m drum Dmax=28.0 mm, Length (m)= 100 + 0 + 0 + 0",4154,"ΤΕΜ",1,"MC",1,"6FX50081BB252AA0"]
["6FX5008-1BB41-1HF0","Power cable sold by the meter type: 6FX5008-1BB41 4x 6.0 C UL/CSA, DESINA MOTION-CONNECT 500 Type of delivery: to 69 m ring from 70 m drum Dmax=13.6 mm, Length (m)= 0 + 70 + 5 + 0",1115,"ΤΕΜ",1,"MC",1,"6FX50081BB411HF0"]
["6FX5008-2DC00-1FA0","Signal cable sold by the meter type: 6FX5008-2DC00 (DRIVE-CLiQ) 2x2X0.22+2x0.38 C UL/CSA DESINA MOTION-CONNECT 500 Type of delivery: Ring Dmax=7.0 mm, Length (m)=50",467,"ΤΕΜ",1,"MC",1,"6FX50082DC001FA0"]
["6FX5012-2CF02-1FA0","Signal cable pre-assembled (resolver in motor) 3x 2x 0.14+4x 0.14+2x0.5 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm Length (m)= TYPE: 6FX5012-2CF02 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = 0 + 50 + 0 + 0",461,"ΤΕΜ",1,"MC",1,"6FX50122CF021FA0"]
["6FX5012-5DN46-1DF0","Power cable pre-assembled TYPE 6FX5012-5DN46 4X4, (2X1.5)C C CONNECTOR SPEED-CONNECT S 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES PREPARED CONDUCTORS, SINAMICS CONNECTOR INCLUDED MOTION-CONNECT 500 UL/CSA, DESINA DMAX=14 MM LENGTH (M) = + 0 + 30 + 5 + 0",652,"ΤΕΜ",1,"MC",1,"6FX50125DN461DF0"]
["6FX7002-5EA41-1DA0","power cable, pre-assembled type: 6FX7002-5EA41 4x 4+(4x 0.5) C, Connector Sz. 1.5 (1FN to 611) trailable UL/CSA DESINA MOTION-CONNECT 700 Dmax=16.6 mm, Length (m)= 0 + 30 + 0 + 0",1065,"ΤΕΜ",1,"MC",1,"6FX70025EA411DA0"]
["6FX7002-5LM82-1AA5","Power cable pre-assembled type: 6FX7002-5LM82 4x 6 C M32/1FN3 screw connection Connector full thread Sz. 1.5 the converter side for SIMODRIVE/MASTERDRIVES MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=14.9 mm Length (m)= 0 0 0 + 0,5",360,"ΤΕΜ",1,"MC",1,"6FX70025LM821AA5"]
["6FX7008-1BC21-1FA0","Power cable sold by the meter type: 6FX7008-1BC21 4x 2.5+4x 0.5 C for linear motors trailable UL/CSA DESINA MOTION-CONNECT 700 Type of delivery: Ring Dmax=15.2 mm, Length (m)=50",1467,"ΤΕΜ",1,"MC",1,"6FX70081BC211FA0"]
["6FX8002-2AH11-1CF0","Signal cable pre-assembled (basic 6FX8002-2AH00-....) with integrated temperature cores trailable UL/CSA DESINA MOTION-CONNECT 800 Dmax=9.3 mm TYPE: 6FX8002-2AH11 LENGTH (M) = 0 + 20 + 5 + 0",370,"ΤΕΜ",1,"MC",1,"6FX80022AH111CF0"]
["6FX8002-2CA11-1CH0","Signal cable pre-assembled for incremental encoder sin/cos 1 Vpp 6FX2001-3 4x (2x0.34)+4x 0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.3 mm Length (m)= TYPE: 6FX8002-2CA11 LENGTH (M) = + 0 + 20 + 7 + 0",334,"ΤΕΜ",1,"MC",1,"6FX80022CA111CH0"]
["6FX8002-2CA31-1CA0","Signal cable pre-assembled for incr. encoder with C/D tracks integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2CA31 LENGTH (M) = + 0 + 20 + 0 + 0",373,"ΤΕΜ",1,"MC",1,"6FX80022CA311CA0"]
["6FX8002-2CA31-1DF0","Signal cable pre-assembled for incr. encoder with C/D tracks integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2CA31 LENGTH (M) = + 0 + 30 + 5 + 0",538,"ΤΕΜ",1,"MC",1,"6FX80022CA311DF0"]
["6FX8002-2CA34-1EA0","Signal cable extension for base 2CA31-2CA80 or -2CA88 3x (2x0.14) C + 4x 0.14+2x0.5+4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2CA34 LENGTH (M) = 0 + 40 + 0 + 0",618,"ΤΕΜ",1,"MC",1,"6FX80022CA341EA0"]
["6FX8002-2CB54-1CD0","signal cable, pre-assembled Extension for incremental encoder TTL 5V, 6FX2001-2 4x (2x0.34)+4x 0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.3 mm Length (m)= TYPE: 6FX8002-2CB54 LENGTH (M) = 0 + 20 + 3 + 0",317,"ΤΕΜ",1,"MC",1,"6FX80022CB541CD0"]
["6FX8002-2CD24-1BA0","Signal cable pre-assembled for incremental encoder TTL RS422 24 V DC, 6FX2001-2 4x (2x0.34)+4x 0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.3 mm Length (m)= TYPE: 6FX8002-2CD24 LENGTH (M) = 0 + 10 + 0 + 0",204,"ΤΕΜ",1,"MC",1,"6FX80022CD241BA0"]
["6FX8002-2CG00-1BE0","Signal cable pre-assembled for incremental encoder SIN/COS 1VPP, 6FX2001-3 4x (2x0.34)+4x 0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.3 mm Length (m)= TYPE: 6FX8002-2CG00 LENGTH (M) = 0 + 10 + 4 + 0",225,"ΤΕΜ",1,"MC",1,"6FX80022CG001BE0"]
["6FX8002-2CP00-1AH0","Signal cable pre-assembled type: 6FX8002-2CP00 for handwheel 840D on COM board 4x (2x0.18) C MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=6.7 mm Length (m)= 0 + 0 + 7 + 0",135,"ΤΕΜ",1,"MC",1,"6FX80022CP001AH0"]
["6FX8002-2DC00-1BG0","Signal cable pre-assembled type: 6FX8002-2DC00 DRIVE-CLiQ with 24 V Connector RJ45 IP20 on both sides MOTION-CONNECT 800PLUS released only up to 75 m length Dmax=7.1 mm Length (m)= 0 + 10 + 6 + 0",306,"ΤΕΜ",1,"MC",1,"6FX80022DC001BG0"]
["6FX8002-2DC10-1BE4","signal cable, pre-assembled type: 6FX8002-2DC10 DRIVE-CLiQ with 24 V Connector RJ45 IP20 on module side and IP67 on motor side MOTION-CONNECT 800PLUS released only up to 75 m length Dmax=7.1 mm Length (m)= 0 + 10 + 4 + 0,4",260,"ΤΕΜ",1,"MC",1,"6FX80022DC101BE4"]
["6FX8002-2DC10-1CF0","signal cable, pre-assembled type: 6FX8002-2DC10 DRIVE-CLiQ with 24 V Connector RJ45 IP20 on module side and IP67 on motor side MOTION-CONNECT 800PLUS released only up to 75 m length Dmax=7.1 mm Length (m)= 0 + 20 + 5 + 0",346,"ΤΕΜ",1,"MC",1,"6FX80022DC101CF0"]
["6FX8002-2DC10-1HG0","signal cable, pre-assembled type: 6FX8002-2DC10 DRIVE-CLiQ with 24 V Connector RJ45 IP20 on module side and IP67 on motor side MOTION-CONNECT 800PLUS released only up to 75 m length Dmax=7.1 mm Length (m)= 0 + 70 + 6 + 0",784,"ΤΕΜ",1,"MC",1,"6FX80022DC101HG0"]
["6FX8002-2DC36-1AD0","Signal cable pre-assembled type: 6FX8002-2DC36 DRIVE-CLiQ with 24 V M12 female/ RJ45 IP67 MOTION-CONNECT 800PLUS UL/CSA, DESINA, Trailable Dmax=7.1 mm Length (m)=3",186,"ΤΕΜ",1,"MC",1,"6FX80022DC361AD0"]
["6FX8002-2DC38-1CA0","Drive-CLiQ adapter cable pre-fabricated Type: 6FX8002-2DC38 DRIVE-CLiQ with 24 V M12 male/ RJ45 IP67 MOTION-CONNECT 800PLUS MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=7.1 mm Length (m)=20",340,"ΤΕΜ",1,"MC",1,"6FX80022DC381CA0"]
["6FX8002-2EN20-1CA0","Signal cable pre-assembled for absolute encoder EnDat in motor AH20 with connector SPEED-CONNECT M17 (3x 2x 0.14) C+4x 0.14+2x 0.5+4x 0.22 C MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2EN20 LENGTH (M) = 0 + 20 + 0 + 0",402,"ΤΕΜ",1,"MC",1,"6FX80022EN201CA0"]
["6FX8002-2EQ10-1FB0","Signal cable pre-assembled for absolute encoder EnDat integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2EQ10 LENGTH (M) = 0 + 50 + 1 + 0",716,"ΤΕΜ",1,"MC",1,"6FX80022EQ101FB0"]
["6FX8002-2EQ18-1BA5","Signal cable pre-assembled for absolute encoder EnDat integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector with set screw MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2EQ18 LENGTH (M) = 0 + 10 + 0 + 0.5",344,"ΤΕΜ",1,"MC",1,"6FX80022EQ181BA5"]
["6FX8002-2SL01-1AF0","Signal cable pre-assembled type: 6FX8002-2SL01 for temperature sensor 3x 2x 0.5+1x 1 C Motor terminals on M17 female VG with screw coupling M20 (K) MOTION-CONNECT 800PLUS UL/CSA, DESINA, Trailable Dmax=11 mm Length (m)= 0 + 0 + 5 + 0",303,"ΤΕΜ",1,"MC",1,"6FX80022SL011AF0"]
["6FX8002-2YW13-1BB6","Signal cable pre-assembled type: 6FX8002-2YW13 Customer-specific Length (m)=",497,"ΤΕΜ",1,"MC",1,"6FX80022YW131BB6"]
["6FX8002-5CA38-1CF0","power cable extension 4x 2.5 C Connector full thread Sz. 1.5 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=11 mm Length (m)= TYPE: 6FX8002-5CA38 LENGTH (M) = 0 + 20 + 5 + 0",780,"ΤΕΜ",1,"MC",1,"6FX80025CA381CF0"]
["6FX8002-5CA68-1CA0","power cable extension 4x 10 C Connector full thread Sz. 1.5 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=18.2 mm Length (m)= TYPE: 6FX8002-5CA68 LENGTH (M) = 0 + 20 + 0 + 0",1126,"ΤΕΜ",1,"MC",1,"6FX80025CA681CA0"]
["6FX8002-5CG01-1CA0","Power cable pre-assembled type: 6FX8002-5CG01 4x 1.5 C, connector Full-thread, size 1 for SINAMICS S120 Power Module MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.5 mm, Length (m)= 0 + 20 + 0 + 0",396,"ΤΕΜ",1,"MC",1,"6FX80025CG011CA0"]
["6FX8002-5CG22-1AH0","Power cable pre-assembled 4x 1.5 C, SPEED-CONNECT Sz. 1.5 for SINAMICS S120 Power Module MOTION-CONNECT 800PLUS Trailable UL/CSA, DESINA Dmax=9.5 mm, Length (m)= TYPE: 6FX8002-5CG22 LENGTH (M) = + 0 + 0 + 7 + 0",307,"ΤΕΜ",1,"MC",1,"6FX80025CG221AH0"]
["6FX8002-5CN05-1BA0","power cable extension 4x 1.5 C, SPEED-CONNECT Sz. 1 MOTION-CONNECT 800PLUS Trailable UL/CSA, DESINA Dmax=9.5 mm TYPE: 6FX8002-5CN05 LENGTH (M) = + 0 + 10 + 0 + 0",380,"ΤΕΜ",1,"MC",1,"6FX80025CN051BA0"]
["6FX8002-5CN06-1BH0","Power cable pre-assembled TYPE 6FX8002-5CN06 4X1,5 C, SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=9.5 MM LENGTH (M) = + 0 + 10 + 7 + 0",396,"ΤΕΜ",1,"MC",1,"6FX80025CN061BH0"]
["6FX8002-5CN54-1FA0","Power cable pre-assembled 4x 6 C SPEED-CONNECT connector Sz. 1.5 Ring cable lugs on module side for SINAMICS S120 Motor Module MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=14.9 mm Length (m)= TYPE: 6FX8002-5CN54 LENGTH (M) = + 0 + 50 + 0 + 0",1480,"ΤΕΜ",1,"MC",1,"6FX80025CN541FA0"]
["6FX8002-5CQ48-1DD0","power cable extension 4x 4 C SPEED-CONNECT connector Sz. 1.5 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=12.3 mm Length (m)= TYPE: 6FX8002-5CQ48 LENGTH (M) = 0 + 30 + 3 + 0",1038,"ΤΕΜ",1,"MC",1,"6FX80025CQ481DD0"]
["6FX8002-5CR42-1BA3","Power cable pre-assembled type: 6FX8002-5CR42 4x 10 C, M40 screw connection SINAMICS S120 Power Module MOTION-CONNECT 800 trailable, UL/CSA, DESINA Dmax=19.4 mm, Length (m)= 0 + 10 + 0 + 0,3",601,"ΤΕΜ",1,"MC",1,"6FX80025CR421BA3"]
["6FX8002-5CR52-1AF0","Power cable pre-assembled type: 6FX8002-5CR52 4x 16 C Screw connection M40/1PH813 for SINAMICS S120, with bare core ends at module side MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=22.3 mm Length (m)= 0 + 0 + 5 + 0",506,"ΤΕΜ",1,"MC",1,"6FX80025CR521AF0"]
["6FX8002-5CS23-1CD0","Power cable pre-assembled type: 6FX8002-5CS23 4x 16 C Connector full thread Sz. 3 for SINAMICS S120 Motor Module Booksize MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=22.3 mm Length (m)= 0 + 20 + 3 + 0",1756,"ΤΕΜ",1,"MC",1,"6FX80025CS231CD0"]
["6FX8002-5CS46-1DA0","Power cable pre-assembled TYPE 6FX8002-5CS46 4X4C, CONN. FULL THREAD S. 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=12.3 MM LENGTH (M) = + 0 + 30 + 0 + 0",754,"ΤΕΜ",1,"MC",1,"6FX80025CS461DA0"]
["6FX8002-5CX18-1AF0","power cable extension 4x 10 C Connector full thread Sz. 3 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=18.2 mm Length (m)= TYPE: 6FX8002-5CX18 LENGTH (M) = 0 + 0 + 5 + 0",1878,"ΤΕΜ",1,"MC",1,"6FX80025CX181AF0"]
["6FX8002-5DA15-1BC0","power cable extension 4x 2.5+(2x1.5) C C MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=13.8 mm Length (m)= TYPE: 6FX8002-5DA15 LENGTH (M) = 0 + 10 + 2 + 0",501,"ΤΕΜ",1,"MC",1,"6FX80025DA151BC0"]
["6FX8002-5DA48-1BA0","power cable extension 4x 4+(2x1.5) C, Connector Sz. 1.5 Connector full thread Sz. 1.5 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=15.2 mm LΓ¤nge (m)= TYPE: 6FX8002-5DA48 LENGTH (M) = 0 + 10 + 0 + 0",654,"ΤΕΜ",1,"MC",1,"6FX80025DA481BA0"]
["6FX8002-5DG01-1AH0","Power cable pre-assembled type: 6FX8002-5DG01 4x 1.5+(2x1.5) C C, connector Connector full thread Sz. 1 for SINAMICS Power Module MOTION-CONNECT 800PLUS Dmax=12 mm, Length (m)= + 0 + 0 + 7 + 0",276,"ΤΕΜ",1,"MC",1,"6FX80025DG011AH0"]
["6FX8002-5DG12-1DD0","Power cable pre-assembled 4x 2.5+(2x1.5) C C SPEED-CONNECT connector Sz. 1 for SINAMICS S120 Power Module and Motor Mod. Booksize Compact MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=13.8 mm Length (m)= TYPE: 6FX8002-5DG12 LENGTH (M) = 0 + 30 + 3 + 0",804,"ΤΕΜ",1,"MC",1,"6FX80025DG121DD0"]
["6FX8002-5DG31-1BA0","Power cable pre-assembled type: 6FX8002-5DG31 4x 2.5+(2x1.5) C C Connector full thread Sz. 1.5 for SINAMICS S120 Power Module and Motor Mod. Booksize Compact MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=13.8 mm Length (m)= + 0 + 10 + 0 + 0",431,"ΤΕΜ",1,"MC",1,"6FX80025DG311BA0"]
["6FX8002-5DG62-1BA0","Power cable pre-assembled 4x 10+(2x1.5) C C SPEED-CONNECT connector Sz. 1.5 for SINAMICS S120 Power Module and Motor Mod. Booksize Compact MOTION-CONNECT 800PLUS Trailable UL/CSA, DESINA Dmax=20.1 mm LΓ¤nge (m)= TYPE: 6FX8002-5DG62 LENGTH (M) = + 0 + 10 + 0 + 0",777,"ΤΕΜ",1,"MC",1,"6FX80025DG621BA0"]
["6FX8002-5DN05-1AH5","power cable extension 4x 1.5+(2x1.5) C C, connector SPEED-CONNECT Sz. 1 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=12 mm, Length (m)= TYPE: 6FX8002-5DN05 LENGTH (M) = + 0 + 0 + 7 + 0,5",400,"ΤΕΜ",1,"MC",1,"6FX80025DN051AH5"]
["6FX8002-5DN36-1BJ0","Power cable pre-assembled TYPE 6FX8002-5DN36 4X2.5 , (2X1.5)C C CONNECTOR SPEED-CONNECT S. 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=13.8 MM LENGTH (M) = + 0 + 10 + 8 + 0",581,"ΤΕΜ",1,"MC",1,"6FX80025DN361BJ0"]
["6FX8002-5DN54-1AD5","Power cable pre-assembled 4x 6+(2x1.5) C C SPEED-CONNECT connector Sz. 1.5 Ring cable lugs on module side for SINAMICS S120 Motor Module MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=17.3 mm LΓ¤nge (m)= TYPE: 6FX8002-5DN54 LENGTH (M) = + 0 + 0 + 3 + 0,5",370,"ΤΕΜ",1,"MC",1,"6FX80025DN541AD5"]
["6FX8002-5DQ48-1BD0","power cable extension 4x 4+(2x1.5) C C SPEED-CONNECT connector Sz. 1.5 MOTION-CONNECT 800PLUS Trailable UL/CSA, DESINA Dmax=15.2 mm LΓ¤nge (m)= TYPE: 6FX8002-5DQ48 LENGTH (M) = + 0 + 10 + 3 + 0",725,"ΤΕΜ",1,"MC",1,"6FX80025DQ481BD0"]
["6FX8002-5DS16-1AE0","Power cable pre-assembled TYPE 6FX8002-5DS16 4X2.5 , (2X1.5)C C CONNECTOR FULL THREAD SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=13.8 MM LENGTH (M) = + 0 + 0 + 4 + 0",295,"ΤΕΜ",1,"MC",1,"6FX80025DS161AE0"]
["6FX8002-5DS23-1BG0","Power cable pre-assembled type: 6FX8002-5DS23 4x 16+(2x1.5) C C Connector full thread Sz. 3 Ring cable lugs on module side for SINAMICS S120 Motor Module MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=23.8 mm Length (m)= 0 + 10 + 6 + 0",1665,"ΤΕΜ",1,"MC",1,"6FX80025DS231BG0"]
["6FX8002-5DX28-1BD0","power cable extension 4x 16+(2x1.5) C C Connector full thread Sz. 3 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=23.8 mm Length (m)= TYPE: 6FX8002-5DX28 LENGTH (M) = 0 + 10 + 3 + 0",2540,"ΤΕΜ",1,"MC",1,"6FX80025DX281BD0"]
["6FX8002-5DX58-1BA0","power cable extension 4x 50+(2x1.5) C C Connector full thread Sz. 3 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=35 mm Length (m)= TYPE: 6FX8002-5DX58 LENGTH (M) = 0 + 10 + 0 + 0",4238,"ΤΕΜ",1,"MC",1,"6FX80025DX581BA0"]
["6FX8002-7HY00-1DB7","Pre-assembled hybrid cable type: 6FX8002-7HY00 Power and DRIVE-CLiQ Outlet direction NDE/NDE for SINAMICS S120M MOTION-CONNECT 800PLUS Trailing type, UL/CSA DESINA Dmax=15 mm, Length (m)= 0 + 30 + 1 + 0,7",1175,"ΤΕΜ",1,"MC",1,"6FX80027HY001DB7"]
["6FX8002-7HY11-1AB0","Pre-assembled hybrid cable type: 6FX8002-7HY11 Power and DRIVE-CLiQ Outlet direction NDE/DE for SINAMICS S120M MOTION-CONNECT 800PLUS Trailing type, UL/CSA DESINA Dmax=15 mm, Length (m)= 0 + 0 + 1 + 0",418,"ΤΕΜ",1,"MC",1,"6FX80027HY111AB0"]
["6FX8002-7HY22-1CE7","Pre-assembled hybrid cable type: 6FX8002-7HY22 Power and DRIVE-CLiQ Outlet direction DE/DE for SINAMICS S120M MOTION-CONNECT 800PLUS Trailing type, UL/CSA DESINA Dmax=15 mm, Length (m)= 0 + 20 + 4 + 0,7",1004,"ΤΕΜ",1,"MC",1,"6FX80027HY221CE7"]
["6FX8005-0BY11-0PK2","CABLE INLET SET 20/40 PRO K2 6FX8005-0BY11 FIRM BYSTRONIC PARTS LIST NUMBER: 10044317 CONSISTING OF: 6FX8002-5CS01-1CC0 - 10030117 6FX8002-2DC10-1CC0 - 10030132 6FX8002-5DS01-1CC0 - 10030136 6FX8002-2DC10-1CC0 - 10030132",2208,"ΤΕΜ",1,"MC",1,"6FX80050BY110PK2"]
["6FX8008-1BA35-1BK0","Power cable sold by the meter type: 6FX8008-1BA35 4x 35+(2x1.5) C C trailable UL/CSA DESINA MOTION-CONNECT 800PLUS Type of delivery: up to 14 m ring from 15 m drum Dmax=31.9 mm Length (m)= 0 + 10 + 9 + 0",2628,"ΤΕΜ",1,"MC",1,"6FX80081BA351BK0"]
["6FX8008-1BB41-1BD0","Power cable sold by the meter type: 6FX8008-1BB41 4x 6.0 C trailable UL/CSA DESINA MOTION-CONNECT 800PLUS Type of delivery: to 69 m ring from 70 m drum Dmax=14.9 mm, Length (m)= 0 + 10 + 3 + 0",354,"ΤΕΜ",1,"MC",1,"6FX80081BB411BD0"]
["6FX8008-1BB61-1AB0","Power cable sold by the meter type: 6FX8008-1BB61 4x 16 C MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=22.3 mm Type of delivery: to 59 m ring from 60 m drum Length (m)= 0 + 0 + 1 + 0",64,"ΤΕΜ",1,"MC",1,"6FX80081BB611AB0"]
["6FX8008-1XB11-2AA0","Power cable sold by the meter type: 6FX8008-1x B11 4x 1.5 C customer-specific MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.5 mm, Length (m)=100 Type of delivery: Disposable drum",1486,"ΤΕΜ",1,"MC",1,"6FX80081XB112AA0"]
["6FX8012-2EQ10-1BJ0","Signal cable pre-assembled for absolute encoder EnDat integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8012-2EQ10 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = 0 + 10 + 8 + 0",351,"ΤΕΜ",1,"MC",1,"6FX80122EQ101BJ0"]
["6FX8012-5CN26-1AJ0","Power cable pre-assembled TYPE 6FX8012-5CN26 4X1,5C, SPEED-CONNECT SIZE 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES PREPARED CONDUCTORS, SINAMICS CONNECTOR INCLUDED MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=9.5 MM LENGTH (M) = + 0 + 0 + 8 + 0",359,"ΤΕΜ",1,"MC",1,"6FX80125CN261AJ0"]
["6FX8022-5CN06-1CC0","Power cable pre-assembled TYPE 6FX8022-5CN06 4X1,5 C, SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES PREPARED CONDUCTORS, W/O SINAMICS CONNECTOR MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=9.5 MM LENGTH (M) = + 0 + 20 + 2 + 0",418,"ΤΕΜ",1,"MC",1,"6FX80225CN061CC0"]
["6FX8022-5DN06-1BA0","Power cable pre-assembled TYPE 6FX8022-5DN06 4X1,5 , (2X1.5)C C CONNECTOR SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES PREPARED CONDUCTORS, W/O SINAMICS CONNECTOR MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=12 MM + 0 + 10 + 0 + 0",337,"ΤΕΜ",1,"MC",1,"6FX80225DN061BA0"]
["6SE6400-3TD11-5FD0","MICROMASTER 4 Output LC filter 380-480V 3AC 112.2/90.0 A (40/50 Β°C) Stand-alone FS E/F 460x 360x 235 (HxWxD)",3332,"ΤΕΜ",1,"MC",1,"6SE64003TD115FD0"]
["6SE6420-2AB11-2AA1","MICROMASTER 420 Built-in Class A filter 200-240V1AC+10/-10% 47-63Hz Constant torque 0.12 kW Overload 150% for 60s Square-law torque 0.12 kW 173x 73x 149 (HxWxD) Degree of protection IP20 Ambient temperature -10+50 Β°C without AOP/BOP",422,"ΤΕΜ",1,"MC",1,"6SE64202AB112AA1"]
["6SE6440-2UC27-5DA1","MICROMASTER 440 WITHOUT FILTER 3AC 200-240 V +10/-10% 47-63 HZ CONSTANT TORQUE POWER 7.5 KW OVERLOAD 150% 60 S, 200% 3 S SQUARED TORQUE POWER 11 KW 520 X 275 X 245 (H X W X D) PROTECTION IP20 AMBIENT TEMP. -10 TO +50 DEG. C WITHOUT AOP/BOP",2272,"ΤΕΜ",1,"MC",1,"6SE64402UC275DA1"]
["6SL3000-0BE34-4AA0","SINAMICS/MICROMASTER PX LINE FILTER INPUT: 3AC 380-480 V, 50/60 HZ 440 A",3709,"ΤΕΜ",1,"MC",1,"6SL30000BE344AA0"]
["6SL3000-2DE32-6EA0","SINAMICS DU/DT filter compact plus voltage peak limiter for Power Module/Motor Module 110/132 kW, 380-480V 3AC max. cable length 100/150 m",4002,"ΤΕΜ",1,"MC",1,"6SL30002DE326EA0"]
["6SL3000-2DH35-8AA0","SINAMICS DU/DT filter plus Voltage peak limiter for Power Module/Motor Module 560kW, 500-690V 3AC max. cable length 300/450 m",12858,"ΤΕΜ",1,"MC",1,"6SL30002DH358AA0"]
["6SL3077-0AA00-4AB0","SINAMICS Technology Extension PARAMBUF Parameter Buffer SOFTWARE OPTION FROM FIRMWARE V4.3 DELIVERY OF ONE LICENSE ON PAPER MACHINE-SPECIFIC DELIVERY RELEASE !",224,"ΤΕΜ",1,"MC",1,"6SL30770AA004AB0"]
["6SL3136-6AE21-0AA1","SINAMICS S120 SMART LINE MODULE INPUT: 3-PH 380-480 V, 50/60 HZ OUTPUT: 600 V DC, 17 A, 10 KW FRAME SIZE: BOOKSIZE COLD PLATE COOLING INCL. CONTROL VOLTAGE ADAPTER.",1785,"ΤΕΜ",1,"MC",1,"6SL31366AE210AA1"]
["6SL3200-0SF14-0AA0","SINAMICS G120/G120C FAN UNIT FSC INCLUDES PLUGABLE FRAME WITH BUILT IN FAN USED FOR PM2X0-2 UND G120C",316,"ΤΕΜ",1,"MC",1,"6SL32000SF140AA0"]
["6SL3200-0WT01-0AA0","Replacement connector kits for SINAMICS V70/V90 400 V module contains control connector, power connector",29.5,"ΤΕΜ",1,"MC",1,"6SL32000WT010AA0"]
["6SL3210-1KE15-8AP2","SINAMICS G120C RATED POWER 2,2KW WITH 150% OVERLOAD FOR 3 SEC 3AC380-480V +10/-20% 47-63HZ INTEGRATED FILTER CLASS A I/O-INTERFACE: 6DI, 2DO,1AI,1AO SAFE TORQUE OFF INTEGRATED FIELDBUS: PROFIBUS-DP PROTECTION: IP20/ UL OPEN TYPE SIZE: FSAA 173X73X155(HXWXD) EXTERNAL 24V",886,"ΤΕΜ",1,"MC",1,"6SL32101KE158AP2"]
["6SL3210-1NE13-1AG1","SINAMICS G120 Power Module PM230 with integrated Class A filter; Degree of protection IP20 380-480 V 3 AC +10/-10% 47-63 Hz Power low overload: 1.1kW at 150% 3s, 110% 57s, 100% 240 s; Ambient temperature 0 to +40 Β°C (LO) 196x 73x 165 (HxWxD), FSA without Control Unit and operating unit released for CU240B/E-2 and CU230P-2 Firmware version V4.4 or higher",398,"ΤΕΜ",1,"MC",1,"6SL32101NE131AG1"]
["6SL3210-1PE21-1UL0","SINAMICS POWER MODULE PM240-2 WITHOUT FILTER WITH BUILT IN BRAKING CHOPPER 3AC380-480V +10/-10% 47-63HZ OUTPUT HIGH OVERLOAD: 3KW FOR 200% 3S,150% 57S,100% 240S AMBIENT TEMP -10 TO +50 DEG C OUTPUT LOW OVERLOAD: 4KW FOR 150% 3S,110% 57S,100% 240S AMBIENT TEMP -10 TO +40 DEG C 291 X 100 X 165 (HXWXD), FSB PROTECTION IP20 WITHOUT CONTROL UNIT AND PANEL APPROVED FOR CU FIRMWARE- VERSION V4.6",860,"ΤΕΜ",1,"MC",1,"6SL32101PE211UL0"]
["6SL3210-5BB21-1BV1","SINAMICS V20 1 AC 200-240 V -10/+10% 47-6 Rated power 1.1 kW with 150% overload for 60 sec. Integrated filter C1 I/O interface: 4 DI, 2 DQ, Fieldbus: USS/Modbus RTU with built-in BOP protection: IP20/ UL open Size: Size AC 160x90x147(HxWxD)",297,"ΤΕΜ",1,"MC",1,"6SL32105BB211BV1"]
["6SL3220-1YC10-0UF0","SINAMICS G120X Rated power: 0.75 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSA Degree of protection IP20 / UL open type Paint finish 3C2 Without operator panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",621,"ΤΕΜ",1,"MC",1,"6SL32201YC100UF0"]
["6SL3220-1YE10-0UP0","SINAMICS G120X Rated power: 0.75 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSA Degree of protection IP20 / UL open type Paint finish 3C2 Without operator panel Without IO expansion Fieldbus integrated: PROFIBUS DP",710,"ΤΕΜ",1,"MC",1,"6SL32201YE100UP0"]
["6SL3220-1YE16-1AB0","SINAMICS G120X Rated power: 2.2 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSA Degree of protection IP20 / UL open type Paint finish 3C2 Without operator panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",871,"ΤΕΜ",1,"MC",1,"6SL32201YE161AB0"]
["6SL3220-1YE26-0AF0","SINAMICS G120X Rated power: 11 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSC Degree of protection IP20 / UL open type Paint finish 3C2 Without operator panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",1808,"ΤΕΜ",1,"MC",1,"6SL32201YE260AF0"]
["6SL3220-1YE42-1AF0","SINAMICS G120X Rated power: 75 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C2 Without operator panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",7522,"ΤΕΜ",1,"MC",1,"6SL32201YE421AF0"]
["6SL3220-1YH22-0AF0","SINAMICS G120X Rated power: 5.5 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C2 Without operator panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",1460,"ΤΕΜ",1,"MC",1,"6SL32201YH220AF0"]
["6SL3220-1YH28-1AB0","SINAMICS G120X Rated power: 15 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C2 Without operator panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",2505,"ΤΕΜ",1,"MC",1,"6SL32201YH281AB0"]
["6SL3220-1YH44-1CB0","SINAMICS G120X Rated power: 90 kW At 110% 60s, 100% 240 s Radio interference suppression filter For category C3 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C2 Without operator panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",9734,"ΤΕΜ",1,"MC",1,"6SL32201YH441CB0"]
["6SL3220-2YC10-1UP0","SINAMICS G120X Rated power: 0.75 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSA Degree of protection IP20 / UL open type Paint finish 3C2 With Basic Operator Panel with IO expansions Fieldbus integrated: PROFIBUS DP",766,"ΤΕΜ",1,"MC",1,"6SL32202YC101UP0"]
["6SL3220-2YE10-1UP0","SINAMICS G120X Rated power: 0.75 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSA Degree of protection IP20 / UL open type Paint finish 3C2 With Basic Operator Panel with IO expansions Fieldbus integrated: PROFIBUS DP",856,"ΤΕΜ",1,"MC",1,"6SL32202YE101UP0"]
["6SL3220-2YE16-0UB0","SINAMICS G120X Rated power: 2.2 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSA Degree of protection IP20 / UL open type Paint finish 3C2 With Basic Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",742,"ΤΕΜ",1,"MC",1,"6SL32202YE160UB0"]
["6SL3220-2YE26-1AF0","SINAMICS G120X Rated power: 11 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSC Degree of protection IP20 / UL open type Paint finish 3C2 With Basic Operator Panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",1954,"ΤΕΜ",1,"MC",1,"6SL32202YE261AF0"]
["6SL3220-2YE52-1AB0","SINAMICS G120X Rated power: 200 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSG Degree of protection IP20 / UL open type Paint finish 3C2 With Basic Operator Panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",15735,"ΤΕΜ",1,"MC",1,"6SL32202YE521AB0"]
["6SL3220-2YE56-0CB0","SINAMICS G120X Rated power: 315 kW at  135% 3 sec or 110% 60 sec, 100% 240 sec; RFI suppression filter  For category C3 3AC380-480V+10/-20% 47-63Hz Ambient temperature 0 to +45 Β°C Size: FSH Degree of protection IP20 / UL open type With Basic Operator Panel Without IO expansion Integrated fieldbus: MODBUS RTU, BACnet MS/TP,USS",21759,"ΤΕΜ",1,"MC",1,"6SL32202YE560CB0"]
["6SL3220-2YH32-1UB0","SINAMICS G120X Rated power: 22 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C2 With Basic Operator Panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",3228,"ΤΕΜ",1,"MC",1,"6SL32202YH321UB0"]
["6SL3220-2YH40-1UP0","SINAMICS G120X Rated power: 55 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSE Degree of protection IP20 / UL open type Paint finish 3C2 With Basic Operator Panel with IO expansions Fieldbus integrated: PROFIBUS DP",6734,"ΤΕΜ",1,"MC",1,"6SL32202YH401UP0"]
["6SL3220-3YC12-1UP0","SINAMICS G120X Rated power: 1.1 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSA Degree of protection IP20 / UL open type Paint finish 3C2 With Intelligent Operator Panel with IO expansions Fieldbus integrated: PROFIBUS DP",870,"ΤΕΜ",1,"MC",1,"6SL32203YC121UP0"]
["6SL3220-3YC32-0UB0","SINAMICS G120X Rated power: 22 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSE Degree of protection IP20 / UL open type Paint finish 3C2 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",3008,"ΤΕΜ",1,"MC",1,"6SL32203YC320UB0"]
["6SL3220-3YE24-0UF0","SINAMICS G120X Rated power: 7.5 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSB Degree of protection IP20 / UL open type Paint finish 3C2 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",1416,"ΤΕΜ",1,"MC",1,"6SL32203YE240UF0"]
["6SL3220-3YE40-1UB0","SINAMICS G120X Rated power: 55 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSE Degree of protection IP20 / UL open type Paint finish 3C2 With Intelligent Operator Panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",5867,"ΤΕΜ",1,"MC",1,"6SL32203YE401UB0"]
["6SL3220-3YE52-1CB0","SINAMICS G120X Rated power: 200 kW At 110% 60s, 100% 240 s Radio interference suppression filter For category C3 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSG Degree of protection IP20 / UL open type Paint finish 3C2 With Intelligent Operator Panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",14060,"ΤΕΜ",1,"MC",1,"6SL32203YE521CB0"]
["6SL3220-3YE58-0CB0","SINAMICS G120X Rated power: 355 kW at  135% 3 sec or 110% 60 sec, 100% 240 sec; RFI suppression filter  For category C3 3AC380-480V+10/-20% 47-63Hz Ambient temperature 0 to +45 Β°C Size: FSH Degree of protection IP20 / UL open type With Intelligent Operator Panel Without IO expansion Integrated fieldbus: MODBUS RTU, BACnet MS/TP,USS",24803,"ΤΕΜ",1,"MC",1,"6SL32203YE580CB0"]
["6SL3220-3YH32-1AB0","SINAMICS G120X Rated power: 22 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C2 With Intelligent Operator Panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",3592,"ΤΕΜ",1,"MC",1,"6SL32203YH321AB0"]
["6SL3220-3YH42-0UP0","SINAMICS G120X Rated power: 75 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C2 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: PROFIBUS DP",7942,"ΤΕΜ",1,"MC",1,"6SL32203YH420UP0"]
["6SL3220-3YH60-1CP0","SINAMICS G120X Rated power: 400 kW at  135% 3 s or 110% 60 s, 100% 240 s; RFI suppression filter  for category C3 3AC500-690V+10/-20% 47-63Hz Ambient temperature 0 to +45 Β°C Size: FSH Degree of protection IP20 / UL open type With Intelligent Operator Panel With IO expansion Fieldbus integrated: PROFIBUS DP",31820,"ΤΕΜ",1,"MC",1,"6SL32203YH601CP0"]
["6SL3230-1YC30-0UF0","SINAMICS G120X Rated power: 18.5 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 Without operator panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",2841,"ΤΕΜ",1,"MC",1,"6SL32301YC300UF0"]
["6SL3230-1YE18-1UB0","SINAMICS G120X Rated power: 3 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSA Degree of protection IP20 / UL open type Paint finish 3C3 Without operator panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",1074,"ΤΕΜ",1,"MC",1,"6SL32301YE181UB0"]
["6SL3230-1YE32-1AB0","SINAMICS G120X Rated power: 22 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 Without operator panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",3388,"ΤΕΜ",1,"MC",1,"6SL32301YE321AB0"]
["6SL3230-1YE44-0UF0","SINAMICS G120X Rated power: 90 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 Without operator panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",8551,"ΤΕΜ",1,"MC",1,"6SL32301YE440UF0"]
["6SL3230-1YE54-0AB0","SINAMICS G120X Rated power: 250 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSG Degree of protection IP20 / UL open type Paint finish 3C3 Without operator panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",20127,"ΤΕΜ",1,"MC",1,"6SL32301YE540AB0"]
["6SL3230-1YH26-1AP0","SINAMICS G120X Rated power: 11 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 Without operator panel with IO expansions Fieldbus integrated: PROFIBUS DP",2428,"ΤΕΜ",1,"MC",1,"6SL32301YH261AP0"]
["6SL3230-1YH38-0UP0","SINAMICS G120X Rated power: 45 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSE Degree of protection IP20 / UL open type Paint finish 3C3 Without operator panel Without IO expansion Fieldbus integrated: PROFIBUS DP",5867,"ΤΕΜ",1,"MC",1,"6SL32301YH380UP0"]
["6SL3230-2YC16-0UF0","SINAMICS G120X Rated power: 2.2 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSB Degree of protection IP20 / UL open type Paint finish 3C3 With Basic Operator Panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",914,"ΤΕΜ",1,"MC",1,"6SL32302YC160UF0"]
["6SL3230-2YC38-1UP0","SINAMICS G120X Rated power: 45 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 With Basic Operator Panel with IO expansions Fieldbus integrated: PROFIBUS DP",5780,"ΤΕΜ",1,"MC",1,"6SL32302YC381UP0"]
["6SL3230-2YE28-0AB0","SINAMICS G120X Rated power: 15 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSC Degree of protection IP20 / UL open type Paint finish 3C3 With Basic Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",2462,"ΤΕΜ",1,"MC",1,"6SL32302YE280AB0"]
["6SL3230-2YE42-1AB0","SINAMICS G120X Rated power: 75 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 With Basic Operator Panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",7902,"ΤΕΜ",1,"MC",1,"6SL32302YE421AB0"]
["6SL3230-2YE50-0CP0","SINAMICS G120X Rated power: 160 kW At 110% 60s, 100% 240 s Radio interference suppression filter For category C3 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSG Degree of protection IP20 / UL open type Paint finish 3C3 With Basic Operator Panel Without IO expansion Fieldbus integrated: PROFIBUS DP",12681,"ΤΕΜ",1,"MC",1,"6SL32302YE500CP0"]
["6SL3230-2YH32-1UP0","SINAMICS G120X Rated power: 22 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 With Basic Operator Panel with IO expansions Fieldbus integrated: PROFIBUS DP",3683,"ΤΕΜ",1,"MC",1,"6SL32302YH321UP0"]
["6SL3230-2YH50-0CB0","SINAMICS G120X Rated power: 160 kW At 110% 60s, 100% 240 s Radio interference suppression filter For category C3 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSG Degree of protection IP20 / UL open type Paint finish 3C3 With Basic Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",14362,"ΤΕΜ",1,"MC",1,"6SL32302YH500CB0"]
["6SL3230-3YC28-1UF0","SINAMICS G120X Rated power: 15 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",2671,"ΤΕΜ",1,"MC",1,"6SL32303YC281UF0"]
["6SL3230-3YC36-0UF0","SINAMICS G120X Rated power: 37 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",4902,"ΤΕΜ",1,"MC",1,"6SL32303YC360UF0"]
["6SL3230-3YE24-0UP0","SINAMICS G120X Rated power: 7.5 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSB Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: PROFIBUS DP",1665,"ΤΕΜ",1,"MC",1,"6SL32303YE240UP0"]
["6SL3230-3YE36-0AB0","SINAMICS G120X Rated power: 37 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",4876,"ΤΕΜ",1,"MC",1,"6SL32303YE360AB0"]
["6SL3230-3YE48-0AP0","SINAMICS G120X Rated power: 132 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: PROFIBUS DP",11852,"ΤΕΜ",1,"MC",1,"6SL32303YE480AP0"]
["6SL3230-3YH26-0UP0","SINAMICS G120X Rated power: 11 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: PROFIBUS DP",2245,"ΤΕΜ",1,"MC",1,"6SL32303YH260UP0"]
["6SL3230-3YH46-0UP0","SINAMICS G120X Rated power: 110 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: PROFIBUS DP",11165,"ΤΕΜ",1,"MC",1,"6SL32303YH460UP0"]
["6SL3260-6AC00-0DA0","SINAMICS G120 Installation frame FSC push-through",71.5,"ΤΕΜ",1,"MC",1,"6SL32606AC000DA0"]
["6SL3310-1GE35-0AA3","SINAMICS G130 Power Module IP20 380-480V 3AC, 50/60 Hz, 490 A Type rating: 250kW 6-pulse supply without power recovery design CIM incl. Drive-CLiQ cable without control module",23886,"ΤΕΜ",1,"MC",1,"6SL33101GE350AA3"]
["6SL3325-1TE32-6AA3","SINAMICS S120 SINGLE MOTOR MODULES INPUT: 600 V DC OUTPUT: 3-PH 400 V, 260 A FRAME SIZE: CHASSIS LIQUID COOLING SUPPORT OF EXTENDED SAFETY INTEGRATED FUNCTIONS",22462,"ΤΕΜ",1,"MC",1,"6SL33251TE326AA3"]
["6SL3544-0LB02-1PA0","SINAMICS G110M Control Unit CU240M DP G PROFIBUS DP with M screw connection 4 DI, 2 DO, 2 AI, 1 F-DI PTC/KTY connection EM brake control Degree of protection IP66 Ambient temperature -10 to +55 Β°C 105x 171x 205 (HxWxD) without Power Module",807,"ΤΕΜ",1,"MC",1,"6SL35440LB021PA0"]
["6SL3544-0TB02-1MA0","SINAMICS G110M Control Unit CU240M AS-Interface Q AS-Interface with plug-in connections for motor frame size 71 4 DI, 2 DO, 2 AI, 1 F-DI PTC/KTY connection EM brake control Degree of protection IP65 Ambient temperature -10 to +55Β° 105x 205x 171 (HxWxD) without Power Module",642,"ΤΕΜ",1,"MC",1,"6SL35440TB021MA0"]
["6AU1810-0BA45-0UE0","SIMOTION SCOUT and Scout TIA V4.5 Unlock Copy License (UCL) Upgrade package for 1 installation only valid in connection with Unlock Copy License agreement requires previous version Scout UCL basic package",395,"ΤΕΜ",1,"MC",1,"6AU18100BA450UE0"]
["6AU1810-1JA22-1XE0","SIMOTION ENGINEERING SYSTEM DCC SIMOTION V2.2 SP1 UPGRADE LICENSE DCC FOR SIMOTION AND FOR SINAMICS OPTION TO SCOUT V4.3 SP1 AND TO STARTER V4.3 SP1 DELIVERY ON DATA CARRIER DVD INCL: FLOATING LICENSE",327,"ΤΕΜ",1,"MC",1,"6AU18101JA221XE0"]
["1MB1011-0EA03-4HA4","SIMOTICS XP Motor type: 1AV2090A Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP65 temperature class 155(F) according to 130(B) Aluminum housing High Efficiency IE2 2-pole * Size 90S * 1.5kW (50 Hz) 1.75 kW (60 Hz) Version for Zone 21 and Zone 22 with conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V3, flange: FF165 (A200) without motor protection Terminal box at top",421,"ΤΕΜ",1,"LVM",1,"1MB10110EA034HA4"]
["1MB1011-1AA42-2AA4","SIMOTICS XP Motor type: 1AV2104A Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP65 temperature class 155(F) according to 130(B) Aluminum housing High Efficiency IE2 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) Version for Zone 21 and Zone 22 with conductive dust 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 without motor protection Terminal box at top",566,"ΤΕΜ",1,"LVM",1,"1MB10111AA422AA4"]
["1MB1011-1CA03-4HB4","SIMOTICS XP Motor type: 1AV2130A Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP65 temperature class 155(F) according to 130(B) Aluminum housing High Efficiency IE2 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) Version for Zone 21 and Zone 22 with conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V3, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",966,"ΤΕΜ",1,"LVM",1,"1MB10111CA034HB4"]
["1MB1011-1DC42-2AB4","SIMOTICS XP Motor type: 1AV2164C Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP65 temperature class 155(F) according to 130(B) Aluminum housing High Efficiency IE2 6-pole * Size 160L, * 11kW (50 Hz) 12.6kW (60 Hz) Version for Zone 21 and Zone 22 with conductive dust 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2062,"ΤΕΜ",1,"LVM",1,"1MB10111DC422AB4"]
["1MB1011-1DC43-4FA4","SIMOTICS XP Motor type: 1AV2164C Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP65 temperature class 155(F) according to 130(B) Aluminum housing High Efficiency IE2 6-pole * Size 160L, * 11kW (50 Hz) 12.6kW (60 Hz) Version for Zone 21 and Zone 22 with conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF300 (A350) without motor protection Terminal box at top",2058,"ΤΕΜ",1,"LVM",1,"1MB10111DC434FA4"]
["1MB1013-0EA43-4FB4","SIMOTICS XP Motor type: 1AV3094A Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP65 temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3 2-pole * Size 90L * 2.2kW (50 Hz) 2.55 (60 Hz) Version for Zone 21 and Zone 22 with conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF165 (A200) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",599,"ΤΕΜ",1,"LVM",1,"1MB10130EA434FB4"]
["1MB1013-1BB23-4HB4","SIMOTICS XP Motor type: 1AV3112B Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP65 temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3 4-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) Version for Zone 21 and Zone 22 with conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V3, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",879,"ΤΕΜ",1,"LVM",1,"1MB10131BB234HB4"]
["1MB1013-1DA22-2HB4","SIMOTICS XP Motor type: 1AV3162A Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP65 temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) Version for Zone 21 and Zone 22 with conductive dust 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V3, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1697,"ΤΕΜ",1,"LVM",1,"1MB10131DA222HB4"]
["1MB1021-0DA23-4FA4","SIMOTICS XP Motor type: 1AV2082A Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) Aluminum housing High Efficiency IE2 2-pole * Size 80M * 0.75kW (50 Hz) 0.86kW (60 Hz) Version for Zone 22 for non-conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF165 (A200) without motor protection Terminal box at top",286,"ΤΕΜ",1,"LVM",1,"1MB10210DA234FA4"]
["1MB1021-0EA42-2FA4","SIMOTICS XP Motor type: 1AV2094A Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) Aluminum housing High Efficiency IE2 2-pole * Size 90L * 2.2kW (50 Hz) 2.55 (60 Hz) Version for Zone 22 for non-conductive dust 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B5, flange: FF165 (A200) without motor protection Terminal box at top",458,"ΤΕΜ",1,"LVM",1,"1MB10210EA422FA4"]
["1MB1021-1BB23-4FA4","SIMOTICS XP Motor type: 1AV2112B Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) Aluminum housing High Efficiency IE2 4-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) Version for Zone 22 for non-conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF215 (A250) without motor protection Terminal box at top",696,"ΤΕΜ",1,"LVM",1,"1MB10211BB234FA4"]
["1MB1021-1DA22-2FA4","SIMOTICS XP Motor type: 1AV2162A Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) Aluminum housing High Efficiency IE2 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) Version for Zone 22 for non-conductive dust 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B5, flange: FF300 (A350) without motor protection Terminal box at top",1410,"ΤΕΜ",1,"LVM",1,"1MB10211DA222FA4"]
["1MB1023-0DA32-2FA4","SIMOTICS XP Motor type: 1AV3083A Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3 2-pole * Size 80M * 1.1kW (50 Hz) 1.27kW (60 Hz) Version for Zone 22 for non-conductive dust 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B5, flange: FF165 (A200) without motor protection Terminal box at top",369,"ΤΕΜ",1,"LVM",1,"1MB10230DA322FA4"]
["1MB1023-0EC02-2AA4","SIMOTICS XP Motor type: 1AV3090C Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3 6-pole * Size 90S * 0.75kW (50 Hz) 0.86kW (60 Hz) Version for Zone 22 for non-conductive dust 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 without motor protection Terminal box at top",383,"ΤΕΜ",1,"LVM",1,"1MB10230EC022AA4"]
["1MB1023-1AC42-2AA4","SIMOTICS XP Motor type: 1AV3104C Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3 60 Hz, P60: IE2 6-pole * Size 100L * 1.5kW (50 Hz) 1.75 kW (60 Hz) Version for Zone 22 for non-conductive dust 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 without motor protection Terminal box at top",517,"ΤΕΜ",1,"LVM",1,"1MB10231AC422AA4"]
["1MB1023-1CA02-2HA4","SIMOTICS XP Motor type: 1AV3130A Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) Version for Zone 22 for non-conductive dust 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V3, flange: FF265 (A300) without motor protection Terminal box at top",911,"ΤΕΜ",1,"LVM",1,"1MB10231CA022HA4"]
["1MB1023-1DA32-2AB4","SIMOTICS XP Motor type: 1AV3163A Low-voltage motor, IEC squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) Version for Zone 22 for non-conductive dust 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1979,"ΤΕΜ",1,"LVM",1,"1MB10231DA322AB4"]
["1MB1031-0DB32-2AB4","SIMOTICS XP Motor type: 1AV2083B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2 4-pole * Size 80M * 0.75 kW (50 Hz) 0.86 kW (60 Hz) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",320,"ΤΕΜ",1,"LVM",1,"1MB10310DB322AB4"]
["1MB1031-0EC43-4AB4","SIMOTICS XP Motor type: 1AV2094C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2 6-pole * Size 90L * 1.1 kW (50 Hz) 1.27 kW (60 Hz) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",437,"ΤΕΜ",1,"LVM",1,"1MB10310EC434AB4"]
["1MB1031-1CB22-2FA4","SIMOTICS XP Motor type: 1AV2132B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2 4-pole * Size 132M, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B5, flange: FF265 (A300) without motor protection Terminal box at top",1117,"ΤΕΜ",1,"LVM",1,"1MB10311CB222FA4"]
["1MB1031-1DA33-4FA4","SIMOTICS XP Motor type: 1AV2163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2 2-pole * Size 160M, * 15 kW (50 Hz) 17.3 kW (60 Hz) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF300 (A350) without motor protection Terminal box at top",1808,"ΤΕΜ",1,"LVM",1,"1MB10311DA334FA4"]
["1MB1033-0DA33-4HB4","SIMOTICS XP Motor type: 1AV3083A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing Premium Efficiency IE3 2-pole * Size 80M * 1.1 kW (50 Hz) 1.27 kW (60 Hz) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V3, flange: FF165 (A200) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",407,"ΤΕΜ",1,"LVM",1,"1MB10330DA334HB4"]
["1MB1033-0EC42-2HB4","SIMOTICS XP Motor type: 1AV3094C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing Premium Efficiency IE3 6-pole * Size 90L * 1.1 kW (50 Hz) 1.27 kW (60 Hz) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V3, flange: FF165 (A200) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",529,"ΤΕΜ",1,"LVM",1,"1MB10330EC422HB4"]
["1MB1033-1CB03-4AA4","SIMOTICS XP Motor type: 1AV3130B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing Premium Efficiency IE3 4-pole * Size 132S, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 without motor protection Terminal box at top",947,"ΤΕΜ",1,"LVM",1,"1MB10331CB034AA4"]
["1MB1033-1CB03-4FB4","SIMOTICS XP Motor type: 1AV3130B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing Premium Efficiency IE3 4-pole * Size 132S, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1080,"ΤΕΜ",1,"LVM",1,"1MB10331CB034FB4"]
["1MB1033-1DB23-4FA4","SIMOTICS XP Motor type: 1AV3162B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing Premium Efficiency IE3 4-pole * Size 160M, * 11 kW (50 Hz) 12.6 kW (60 Hz) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF300 (A350) without motor protection Terminal box at top",1620,"ΤΕΜ",1,"LVM",1,"1MB10331DB234FA4"]
["1MB1511-0EB42-2FB4","SIMOTICS XP Motor type: 1CV2094B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP65 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 4-pole *Size 90L * 1.5 kW (1500 rpm) EX TB IIIC T120Β°DB Version for Zone 21 and Zone 22 with conductive dust 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM B 5, flange: FF165 (A200) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",538,"ΤΕΜ",1,"LVM",1,"1MB15110EB422FB4"]
["1MB1511-1BB22-2FA4","SIMOTICS XP Motor type: 1CV2112B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP65 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2 4-pole * Size 112M, * 4 kW (50 Hz) 4.55 kW (60 Hz) EX TB IIIC T120Β°DB Version for Zone 21 and Zone 22 with conductive dust 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM B5, flange: FF215 (A250) without motor protection Terminal box at top",797,"ΤΕΜ",1,"LVM",1,"1MB15111BB222FA4"]
["1MB1511-1CB22-2FB4","SIMOTICS XP Motor type: 1CV2132B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP65 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2 4-pole * Size 132M, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) EX TB IIIC T120Β°DB Version for Zone 21 and Zone 22 with conductive dust 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM B5, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1299,"ΤΕΜ",1,"LVM",1,"1MB15111CB222FB4"]
["1MB1513-0DA33-4AA4","SIMOTICS XP Motor type: 1CV3083A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP65 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE3, 2-pole *Size 80M * 1.1 kW (3000 rpm) EX TB IIIC T120Β°DB Version for Zone 21 and Zone 22 with conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 without motor protection Terminal box at top",474,"ΤΕΜ",1,"LVM",1,"1MB15130DA334AA4"]
["1MB1513-0EB02-2HA4","SIMOTICS XP Motor type: 1CV3090B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP65 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE3, 4-pole *Size 90S * 1.1 kW (1500 rpm) EX TB IIIC T120Β°DB Version for Zone 21 and Zone 22 with conductive dust 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM V 3, flange: FF165 (A200) without motor protection Terminal box at top",567,"ΤΕΜ",1,"LVM",1,"1MB15130EB022HA4"]
["1MB1513-1CA02-2AA4","SIMOTICS XP Motor type: 1CV3130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP65 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3 2-pole * Size 132S, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) EX TB IIIC T120Β°DB Version for Zone 21 and Zone 22 with conductive dust 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM B3 without motor protection Terminal box at top",973,"ΤΕΜ",1,"LVM",1,"1MB15131CA022AA4"]
["1MB1513-1CA12-2HA4","SIMOTICS XP Motor type: 1CV3131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP65 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3 2-pole * Size 132S, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) EX TB IIIC T120Β°DB Version for Zone 21 and Zone 22 with conductive dust 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM V3, flange: FF265 (A300) without motor protection Terminal box at top",1266,"ΤΕΜ",1,"LVM",1,"1MB15131CA122HA4"]
["1MB1521-0DA22-2HB4","SIMOTICS XP Motor type: 1CV2082A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 2-pole *Size 80M * 0.75 kW (3000 rpm) EX TC IIIB T120Β° DC Version for Zone 22 for non-conductive dust 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM V 3, flange: FF165 (A200) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",351,"ΤΕΜ",1,"LVM",1,"1MB15210DA222HB4"]
["1MB1521-0DC33-4FB4","SIMOTICS XP Motor type: 1CV2083C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 6-pole *Size 80M * 0.55 kW (1000 rpm) EX TC IIIB T120Β° DC Version for Zone 22 for non-conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF165 (A200) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",383,"ΤΕΜ",1,"LVM",1,"1MB15210DC334FB4"]
["1MB1521-0EC43-4AB4","SIMOTICS XP Motor type: 1CV2094C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 6-pole *Size 90L * 1.1 kW (1000 rpm) EX TC IIIB T120Β° DC Version for Zone 22 for non-conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",462,"ΤΕΜ",1,"LVM",1,"1MB15210EC434AB4"]
["1MB1521-1CA12-2FB4","SIMOTICS XP Motor type: 1CV2131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2 2-pole * Size 132S, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) EX TC IIIB T120Β° DC Version for Zone 22 for non-conductive dust 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM B5, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1168,"ΤΕΜ",1,"LVM",1,"1MB15211CA122FB4"]
["1MB1523-0DA22-2FB4","SIMOTICS XP Motor type: 1CV3082A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE3, 2-pole *Size 80M * 0.75 kW (3000 rpm) EX TC IIIB T120Β° DC Version for Zone 22 for non-conductive dust 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM B 5, flange: FF165 (A200) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",420,"ΤΕΜ",1,"LVM",1,"1MB15230DA222FB4"]
["1MB1523-0EB43-4AA4","SIMOTICS XP Motor type: 1CV3094B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE3, 4-pole *Size 90L * 1.5 kW (1500 rpm) EX TC IIIB T120Β° DC Version for Zone 22 for non-conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 without motor protection Terminal box at top",544,"ΤΕΜ",1,"LVM",1,"1MB15230EB434AA4"]
["1MB1523-1BB22-2HA4","SIMOTICS XP Motor type: 1CV3112B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3 4-pole * Size 112M, * 4 kW (50 Hz) 4.55 kW (60 Hz) EX TC IIIB T120Β° DC Version for Zone 22 for non-conductive dust 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM V3, flange: FF215 (A250) without motor protection Terminal box at top",828,"ΤΕΜ",1,"LVM",1,"1MB15231BB222HA4"]
["1MB1523-1CB23-4HB4","SIMOTICS XP Motor type: 1CV3132B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3 4-pole * Size 132M, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) EX TC IIIB T120Β° DC Version for Zone 22 for non-conductive dust 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V3, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1374,"ΤΕΜ",1,"LVM",1,"1MB15231CB234HB4"]
["1MB1531-0DA33-4FB4","SIMOTICS XP Motor type: 1CV2083A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 2-pole *Size 80M * 1.1 kW (3000 rpm) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF165 (A200) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",413,"ΤΕΜ",1,"LVM",1,"1MB15310DA334FB4"]
["1MB1531-0DC23-4AA4","SIMOTICS XP Motor type: 1CV2082C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 6-pole *Size 80M * 0.37 kW (1000 rpm) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 without motor protection Terminal box at top",322,"ΤΕΜ",1,"LVM",1,"1MB15310DC234AA4"]
["1MB1531-0EC03-4HA4","SIMOTICS XP Motor type: 1CV2090C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 6-pole *Size 90S * 0.75 kW (1000 rpm) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 3, flange: FF165 (A200) without motor protection Terminal box at top",437,"ΤΕΜ",1,"LVM",1,"1MB15310EC034HA4"]
["1MB1531-1CA13-4AB4","SIMOTICS XP Motor type: 1CV2131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2 2-pole * Size 132S, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1146,"ΤΕΜ",1,"LVM",1,"1MB15311CA134AB4"]
["1MB1533-0DA23-4AA4","SIMOTICS XP Motor type: 1CV3082A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE3, 2-pole *Size 80M * 0.75 kW (3000 rpm) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 without motor protection Terminal box at top",402,"ΤΕΜ",1,"LVM",1,"1MB15330DA234AA4"]
["1MB1533-0DC32-2HB4","SIMOTICS XP Motor type: 1CV3083C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE3, 6-pole *Size 80M * 0.55 kW (1000 rpm) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM V 3, flange: FF165 (A200) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",479,"ΤΕΜ",1,"LVM",1,"1MB15330DC322HB4"]
["1MB1533-1AB52-2FB4","SIMOTICS XP Motor type: 1CV3105B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3 4-pole * Size 100L * 3 kW (50 Hz) 3.45 kW (60 Hz) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM B5, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",757,"ΤΕΜ",1,"LVM",1,"1MB15331AB522FB4"]
["1MB1533-1CC23-4FA4","SIMOTICS XP Motor type: 1CV3132C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3 6-pole * Size 132M, * 4 kW (50 Hz) 4.55 kW (60 Hz) EX EC IIC T3 GC Version for Zone 2 according to IEC/EN 60 079-7 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF265 (A300) without motor protection Terminal box at top",1165,"ΤΕΜ",1,"LVM",1,"1MB15331CC234FA4"]
["1MB1553-0DB32-1AA4","SIMOTICS XP Motor type: 1CD3083B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE3 4-pole * Size 80M * 0.75 kW (50 Hz) 0.75 kW (60 Hz) Ex db eb IIC T4 Version for Zone 1 3AC 50 Hz 220VD/380VY * 3AC 60 Hz 440VY IM B3 without motor protection Terminal box at top",1344,"ΤΕΜ",1,"LVM",1,"1MB15530DB321AA4"]
["1LE1003-1CC22-2GA7","SIMOTICS GP MOTOR TYPE: 1AV3132C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 132M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF265 (A300) without motor protection Terminal box below",985,"ΤΕΜ",1,"LVM",1,"1LE10031CC222GA7"]
["1LE1003-1CC30-4WB7","SIMOTICS GP MOTOR TYPE: 1AV3133C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 132M, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF265 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1302,"ΤΕΜ",1,"LVM",1,"1LE10031CC304WB7"]
["1LE1003-1CC32-2GC7","SIMOTICS GP MOTOR TYPE: 1AV3133C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 132M, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",1327,"ΤΕΜ",1,"LVM",1,"1LE10031CC322GC7"]
["1LE1003-1CC33-3WB7","SIMOTICS GP MOTOR TYPE: 1AV3133C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 132M, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 15 * Flange: FF265 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1337,"ΤΕΜ",1,"LVM",1,"1LE10031CC333WB7"]
["1LE1003-1CD00-4JA5","SIMOTICS GP MOTOR TYPE: 1AV3130D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 132S, * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF265 (A300) without motor protection Terminal box on RHS",1206,"ΤΕΜ",1,"LVM",1,"1LE10031CD004JA5"]
["1LE1003-1CD03-3GB6","SIMOTICS GP MOTOR TYPE: 1AV3130D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 132S, * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1315,"ΤΕΜ",1,"LVM",1,"1LE10031CD033GB6"]
["1LE1003-1CD22-1JB6","SIMOTICS GP MOTOR TYPE: 1AV3132D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 132M, * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1535,"ΤΕΜ",1,"LVM",1,"1LE10031CD221JB6"]
["1LE1003-1DA20-4JB5","SIMOTICS GP MOTOR TYPE: 1AV3162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",1513,"ΤΕΜ",1,"LVM",1,"1LE10031DA204JB5"]
["1LE1003-1DA22-2GC7","SIMOTICS GP MOTOR TYPE: 1AV3162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",1544,"ΤΕΜ",1,"LVM",1,"1LE10031DA222GC7"]
["1LE1003-1DA23-4AA7","SIMOTICS GP MOTOR TYPE: 1AV3162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VY IM B3 Without motor protection Terminal box below",1358,"ΤΕΜ",1,"LVM",1,"1LE10031DA234AA7"]
["1LE1003-1DA23-4JA7","SIMOTICS GP MOTOR TYPE: 1AV3162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VY IM B 35, flange: FF300 (A350) Without motor protection Terminal box below",1437,"ΤΕΜ",1,"LVM",1,"1LE10031DA234JA7"]
["1LE1003-1DA32-2FA5","SIMOTICS GP MOTOR TYPE: 1AV3163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF300 (A350) Without motor protection Terminal box on RHS",1833,"ΤΕΜ",1,"LVM",1,"1LE10031DA322FA5"]
["1LE1003-1DA33-3JB5","SIMOTICS GP MOTOR TYPE: 1AV3163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 35, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",1959,"ΤΕΜ",1,"LVM",1,"1LE10031DA333JB5"]
["1LE1003-1DA42-1AB6","SIMOTICS GP MOTOR TYPE: 1AV3164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",2203,"ΤΕΜ",1,"LVM",1,"1LE10031DA421AB6"]
["1LE1003-1DA43-3WB4","SIMOTICS GP MOTOR TYPE: 1AV3164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 15 * Flange: FF300 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2249,"ΤΕΜ",1,"LVM",1,"1LE10031DA433WB4"]
["1LE1003-1DA43-4WC7","SIMOTICS GP MOTOR TYPE: 1AV3164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF300 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",2300,"ΤΕΜ",1,"LVM",1,"1LE10031DA434WC7"]
["1LE1003-1DB22-2GC5","SIMOTICS GP MOTOR TYPE: 1AV3162B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",1574,"ΤΕΜ",1,"LVM",1,"1LE10031DB222GC5"]
["1LE1003-1DB23-3JA7","SIMOTICS GP MOTOR TYPE: 1AV3162B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 35, flange: FF300 (A350) Without motor protection Terminal box below",1510,"ΤΕΜ",1,"LVM",1,"1LE10031DB233JA7"]
["1LE1003-1DB42-1JA7","SIMOTICS GP MOTOR TYPE: 1AV3164B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 160L, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35, flange: FF300 (A350) Without motor protection Terminal box below",1909,"ΤΕΜ",1,"LVM",1,"1LE10031DB421JA7"]
["1LE1003-1DB42-2AB7","SIMOTICS GP MOTOR TYPE: 1AV3164B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 160L, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1862,"ΤΕΜ",1,"LVM",1,"1LE10031DB422AB7"]
["1LE1003-1DB43-3JB7","SIMOTICS GP MOTOR TYPE: 1AV3164B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 160L, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 35, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1985,"ΤΕΜ",1,"LVM",1,"1LE10031DB433JB7"]
["1LE1003-1DC22-2FC4","SIMOTICS GP MOTOR TYPE: 1AV3162C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 160M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",1590,"ΤΕΜ",1,"LVM",1,"1LE10031DC222FC4"]
["1LE1003-1DC22-2WB4","SIMOTICS GP MOTOR TYPE: 1AV3162C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 160M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 15 * Flange: FF300 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1580,"ΤΕΜ",1,"LVM",1,"1LE10031DC222WB4"]
["1LE1003-1DC40-4AB7","SIMOTICS GP MOTOR TYPE: 1AV3164C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 160L, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box below",2064,"ΤΕΜ",1,"LVM",1,"1LE10031DC404AB7"]
["1LE1003-1DC42-2FA7","SIMOTICS GP MOTOR TYPE: 1AV3164C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 160L, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF300 (A350) without motor protection Terminal box below",2059,"ΤΕΜ",1,"LVM",1,"1LE10031DC422FA7"]
["1LE1003-1DC43-4GA4","SIMOTICS GP MOTOR TYPE: 1AV3164C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 160L, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) without motor protection Terminal box at top",2004,"ΤΕΜ",1,"LVM",1,"1LE10031DC434GA4"]
["1LE1003-1DD20-4GA6","SIMOTICS GP MOTOR TYPE: 1AV3162D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 160M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) without motor protection Terminal box on left-hand side",1749,"ΤΕΜ",1,"LVM",1,"1LE10031DD204GA6"]
["1LE1003-1DD23-4JC6","SIMOTICS GP MOTOR TYPE: 1AV3162D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 160M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",1872,"ΤΕΜ",1,"LVM",1,"1LE10031DD234JC6"]
["1LE1003-1DD33-3JA4","SIMOTICS GP MOTOR TYPE: 1AV3163D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 160M, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2076,"ΤΕΜ",1,"LVM",1,"1LE10031DD333JA4"]
["1LE1003-1DD40-4GA7","SIMOTICS GP MOTOR TYPE: 1AV3164D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 160L, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) without motor protection Terminal box below",2450,"ΤΕΜ",1,"LVM",1,"1LE10031DD404GA7"]
["1LE1003-1DD42-2AA4","SIMOTICS GP MOTOR TYPE: 1AV3164D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 160L, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 without motor protection Terminal box at top",2323,"ΤΕΜ",1,"LVM",1,"1LE10031DD422AA4"]
["1LE1003-1EA20-4AB5","SIMOTICS GP MOTOR TYPE: 1AV3182A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 180 * 22kW (50 Hz) 24.5kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",2418,"ΤΕΜ",1,"LVM",1,"1LE10031EA204AB5"]
["1LE1003-1EB20-4AA6","SIMOTICS GP MOTOR TYPE: 1AV3182B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 180 * 18.5kW (50 Hz) 21.3kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B3 without motor protection Terminal box on left-hand side",2002,"ΤΕΜ",1,"LVM",1,"1LE10031EB204AA6"]
["1LE1003-1EB40-4GB4","SIMOTICS GP MOTOR TYPE: 1AV3184B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 180 * 22kW (50 Hz) 25.3kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2410,"ΤΕΜ",1,"LVM",1,"1LE10031EB404GB4"]
["1LE1003-1EB43-3AB6","SIMOTICS GP MOTOR TYPE: 1AV3184B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 180 * 22kW (50 Hz) 25.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",2434,"ΤΕΜ",1,"LVM",1,"1LE10031EB433AB6"]
["1LE1003-1EC42-1JA5","SIMOTICS GP MOTOR TYPE: 1AV3184C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 180 * 15kW (50 Hz) 18kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box on RHS",2655,"ΤΕΜ",1,"LVM",1,"1LE10031EC421JA5"]
["1LE1003-1ED40-4AB5","SIMOTICS GP MOTOR TYPE: 1AV3184D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 180 * 11kW (50 Hz) 13.2kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",2997,"ΤΕΜ",1,"LVM",1,"1LE10031ED404AB5"]
["1LE1003-1ED42-2GB6","SIMOTICS GP MOTOR TYPE: 1AV3184D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 180 * 11kW (50 Hz) 13.2kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",3110,"ΤΕΜ",1,"LVM",1,"1LE10031ED422GB6"]
["1LE1003-2AA42-1JB4","SIMOTICS GP MOTOR TYPE: 1AV3204A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 200 * 30kW (50 Hz) 33.5kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",3276,"ΤΕΜ",1,"LVM",1,"1LE10032AA421JB4"]
["1LE1003-2AA50-4GA6","SIMOTICS GP MOTOR TYPE: 1AV3205A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 200 * 37kW (50 Hz) 41.5kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF350 (A400) without motor protection Terminal box on left-hand side",3912,"ΤΕΜ",1,"LVM",1,"1LE10032AA504GA6"]
["1LE1003-2AB53-3AA6","SIMOTICS GP MOTOR TYPE: 1AV3205B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 200 * 30kW (50 Hz) 34.5kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B3 without motor protection Terminal box on left-hand side",3048,"ΤΕΜ",1,"LVM",1,"1LE10032AB533AA6"]
["1LE1003-2AC40-4AB5","SIMOTICS GP MOTOR TYPE: 1AV3204C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 200 * 18.5kW (50 Hz) 22 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",3103,"ΤΕΜ",1,"LVM",1,"1LE10032AC404AB5"]
["1LE1003-2AD50-4AA5","SIMOTICS GP MOTOR TYPE: 1AV3205D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 200 * 15kW (50 Hz) 18kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box on RHS",3788,"ΤΕΜ",1,"LVM",1,"1LE10032AD504AA5"]
["1LE1003-2AD53-3GA5","SIMOTICS GP MOTOR TYPE: 1AV3205D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 200 * 15kW (50 Hz) 18kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF350 (A400) without motor protection Terminal box on RHS",3983,"ΤΕΜ",1,"LVM",1,"1LE10032AD533GA5"]
["1LE1004-1AA42-2AA6","SIMOTICS GP MOTOR TYPE: 1AV4104A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, without motor protection Terminal box on left-hand side",645,"ΤΕΜ",1,"LVM",1,"1LE10041AA422AA6"]
["1LE1004-1AA42-2JA7","SIMOTICS GP MOTOR TYPE: 1AV4104A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF215 (A250) without motor protection Terminal box below",682,"ΤΕΜ",1,"LVM",1,"1LE10041AA422JA7"]
["1LE1004-1AB42-1FB7","SIMOTICS GP MOTOR TYPE: 1AV4104B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 100L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",705,"ΤΕΜ",1,"LVM",1,"1LE10041AB421FB7"]
["1LE1004-1AB42-2AB4","SIMOTICS GP MOTOR TYPE: 1AV4104B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 100L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",605,"ΤΕΜ",1,"LVM",1,"1LE10041AB422AB4"]
["1LE1004-1AB50-4AB4","SIMOTICS GP MOTOR TYPE: 1AV4105B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",685,"ΤΕΜ",1,"LVM",1,"1LE10041AB504AB4"]
["1LE1004-1AB52-1GA5","SIMOTICS GP MOTOR TYPE: 1AV4105B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF215 (A250) without motor protection Terminal box on RHS",735,"ΤΕΜ",1,"LVM",1,"1LE10041AB521GA5"]
["1LE1004-1AB53-4AA5","SIMOTICS GP MOTOR TYPE: 1AV4105B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box on RHS",678,"ΤΕΜ",1,"LVM",1,"1LE10041AB534AA5"]
["1LE1004-1BA20-4JB6","SIMOTICS GP MOTOR TYPE: 1AV4112A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",854,"ΤΕΜ",1,"LVM",1,"1LE10041BA204JB6"]
["1LE1004-1BA22-2GA6","SIMOTICS GP MOTOR TYPE: 1AV4112A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF215 (A250) without motor protection Terminal box on left-hand side",800,"ΤΕΜ",1,"LVM",1,"1LE10041BA222GA6"]
["1LE1004-1BB20-4FA7","SIMOTICS GP MOTOR TYPE: 1AV4112B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF215 (A250) without motor protection Terminal box below",867,"ΤΕΜ",1,"LVM",1,"1LE10041BB204FA7"]
["1LE1004-1BB23-3AA5","SIMOTICS GP MOTOR TYPE: 1AV4112B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 3, without motor protection Terminal box on RHS",852,"ΤΕΜ",1,"LVM",1,"1LE10041BB233AA5"]
["1LE1004-1BB23-4JB7","SIMOTICS GP MOTOR TYPE: 1AV4112B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",921,"ΤΕΜ",1,"LVM",1,"1LE10041BB234JB7"]
["1LE1004-1CA02-2FC6","SIMOTICS GP MOTOR TYPE: 1AV4130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",1117,"ΤΕΜ",1,"LVM",1,"1LE10041CA022FC6"]
["1LE1004-1CA03-3AB4","SIMOTICS GP MOTOR TYPE: 1AV4130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1006,"ΤΕΜ",1,"LVM",1,"1LE10041CA033AB4"]
["1LE1004-1CA03-4WC6","SIMOTICS GP MOTOR TYPE: 1AV4130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF265 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",1132,"ΤΕΜ",1,"LVM",1,"1LE10041CA034WC6"]
["1LE1004-1CA12-1WB4","SIMOTICS GP MOTOR TYPE: 1AV4131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 15 * Flange: FF265 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1315,"ΤΕΜ",1,"LVM",1,"1LE10041CA121WB4"]
["1LE1004-1CA13-4JA5","SIMOTICS GP MOTOR TYPE: 1AV4131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF265 (A300) without motor protection Terminal box on RHS",1244,"ΤΕΜ",1,"LVM",1,"1LE10041CA134JA5"]
["1LE1004-1CB00-4GB5","SIMOTICS GP MOTOR TYPE: 1AV4130B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",1153,"ΤΕΜ",1,"LVM",1,"1LE10041CB004GB5"]
["1LE1004-1CB02-2JC6","SIMOTICS GP MOTOR TYPE: 1AV4130B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",1195,"ΤΕΜ",1,"LVM",1,"1LE10041CB022JC6"]
["1LE1004-1CB20-4AB6","SIMOTICS GP MOTOR TYPE: 1AV4132B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 132M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1354,"ΤΕΜ",1,"LVM",1,"1LE10041CB204AB6"]
["1LE1004-1CB20-4WB7","SIMOTICS GP MOTOR TYPE: 1AV4132B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 132M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF265 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1424,"ΤΕΜ",1,"LVM",1,"1LE10041CB204WB7"]
["1LE1004-1CB22-2GA6","SIMOTICS GP MOTOR TYPE: 1AV4132B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 132M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF265 (A300) without motor protection Terminal box on left-hand side",1334,"ΤΕΜ",1,"LVM",1,"1LE10041CB222GA6"]
["1LE1004-1CB23-4JA4","SIMOTICS GP MOTOR TYPE: 1AV4132B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 132M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF265 (A300) without motor protection Terminal box at top",1284,"ΤΕΜ",1,"LVM",1,"1LE10041CB234JA4"]
["1LE1004-1DA22-2GC4","SIMOTICS GP MOTOR TYPE: 1AV4162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",1766,"ΤΕΜ",1,"LVM",1,"1LE10041DA222GC4"]
["1LE1004-1DA23-3JA5","SIMOTICS GP MOTOR TYPE: 1AV4162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 35 * Flange: FF300 (A350) without motor protection Terminal box on RHS",1758,"ΤΕΜ",1,"LVM",1,"1LE10041DA233JA5"]
["1LE1004-1DA30-4GB5","SIMOTICS GP MOTOR TYPE: 1AV4163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",2261,"ΤΕΜ",1,"LVM",1,"1LE10041DA304GB5"]
["1LE1004-1DA32-2GC6","SIMOTICS GP MOTOR TYPE: 1AV4163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",2300,"ΤΕΜ",1,"LVM",1,"1LE10041DA322GC6"]
["1LE1004-1DA33-4JC4","SIMOTICS GP MOTOR TYPE: 1AV4163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",2253,"ΤΕΜ",1,"LVM",1,"1LE10041DA334JC4"]
["1LE1004-1DA40-4FA4","SIMOTICS GP MOTOR TYPE: 1AV4164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",2529,"ΤΕΜ",1,"LVM",1,"1LE10041DA404FA4"]
["1LE1004-1DA43-3WB5","SIMOTICS GP MOTOR TYPE: 1AV4164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 15 * Flange: FF300 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",2733,"ΤΕΜ",1,"LVM",1,"1LE10041DA433WB5"]
["1LE1004-1DB20-4AB7","SIMOTICS GP MOTOR TYPE: 1AV4162B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1744,"ΤΕΜ",1,"LVM",1,"1LE10041DB204AB7"]
["1LE1004-1DB20-4WB5","SIMOTICS GP MOTOR TYPE: 1AV4162B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF300 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",1845,"ΤΕΜ",1,"LVM",1,"1LE10041DB204WB5"]
["1LE1004-1DB23-3GB4","SIMOTICS GP MOTOR TYPE: 1AV4162B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1804,"ΤΕΜ",1,"LVM",1,"1LE10041DB233GB4"]
["1LE1004-1DB23-4JB6","SIMOTICS GP MOTOR TYPE: 1AV4162B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1824,"ΤΕΜ",1,"LVM",1,"1LE10041DB234JB6"]
["1LE1004-1DB42-2FB4","SIMOTICS GP MOTOR TYPE: 1AV4164B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 160L, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2235,"ΤΕΜ",1,"LVM",1,"1LE10041DB422FB4"]
["1LE1004-1DB43-4WC5","SIMOTICS GP MOTOR TYPE: 1AV4164B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 160L, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF300 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",2359,"ΤΕΜ",1,"LVM",1,"1LE10041DB434WC5"]
["1LE1023-1CA12-2FA4","SIMOTICS GP MOTOR TYPE: 1AV3131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing IE3, NEMA Premium, CSA, UL, 2-pole * Size 132S, * 7.5kW (50 Hz) NEMA 60Hz: 10HP 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF265 (A300) without motor protection Terminal box at top",1110,"ΤΕΜ",1,"LVM",1,"1LE10231CA122FA4"]
["1LE1501-0CA32-2AC4","SIMOTICS SD MOTOR TYPE: 1CV2073A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 2-pole * Size 71M * 0.55kW (50 Hz) 0.63kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 2 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",339,"ΤΕΜ",1,"LVM",1,"1LE15010CA322AC4"]
["1LE1501-1CA12-2GA5","SIMOTICS SD MOTOR TYPE: 1CV2131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF265 (A300) without motor protection Terminal box on RHS",1015,"ΤΕΜ",1,"LVM",1,"1LE15011CA122GA5"]
["1LE1501-1CA13-4JB5","SIMOTICS SD MOTOR TYPE: 1CV2131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",1092,"ΤΕΜ",1,"LVM",1,"1LE15011CA134JB5"]
["1LE1501-1DA42-2JC5","SIMOTICS SD MOTOR TYPE: 1CV2164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations to be considered! 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",2199,"ΤΕΜ",1,"LVM",1,"1LE15011DA422JC5"]
["1LE1501-1EA20-4JB4","SIMOTICS SD MOTOR TYPE: 1CV2182A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 180M, * 22kW (50 Hz) 24.5kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2417,"ΤΕΜ",1,"LVM",1,"1LE15011EA204JB4"]
["1LE1501-1EB20-4FB6","SIMOTICS SD MOTOR TYPE: 1CV2182B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 180M, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",2222,"ΤΕΜ",1,"LVM",1,"1LE15011EB204FB6"]
["1LE1501-1EB22-2FA5","SIMOTICS SD MOTOR TYPE: 1CV2182B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 180M, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF300 (A350) without motor protection Terminal box on RHS",2121,"ΤΕΜ",1,"LVM",1,"1LE15011EB222FA5"]
["1LE1501-1EB23-4JB4","SIMOTICS SD MOTOR TYPE: 1CV2182B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 180M, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2085,"ΤΕΜ",1,"LVM",1,"1LE15011EB234JB4"]
["1LE1501-1EB42-2GB6","SIMOTICS SD MOTOR TYPE: 1CV2184B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 180L, * 22kW (50 Hz) 25.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",2524,"ΤΕΜ",1,"LVM",1,"1LE15011EB422GB6"]
["1LE1501-1EB43-4JA6","SIMOTICS SD MOTOR TYPE: 1CV2184B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 180L, * 22kW (50 Hz) 25.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF300 (A350) without motor protection Terminal box on left-hand side",2443,"ΤΕΜ",1,"LVM",1,"1LE15011EB434JA6"]
["1LE1501-1EC42-1FA4","SIMOTICS SD MOTOR TYPE: 1CV2184C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 6-pole * Size 180L, * 15kW (50 Hz) 18kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",2469,"ΤΕΜ",1,"LVM",1,"1LE15011EC421FA4"]
["1LE1501-1EC43-3GA5","SIMOTICS SD MOTOR TYPE: 1CV2184C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 6-pole * Size 180L, * 15kW (50 Hz) 18kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF300 (A350) without motor protection Terminal box on RHS",2625,"ΤΕΜ",1,"LVM",1,"1LE15011EC433GA5"]
["1LE1501-2AA42-2JC6","SIMOTICS SD MOTOR TYPE: 1CV2204A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 200L, * 30kW (50 Hz) 33.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF350 (A400) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",3368,"ΤΕΜ",1,"LVM",1,"1LE15012AA422JC6"]
["1LE1501-2AA43-3JB6","SIMOTICS SD MOTOR TYPE: 1CV2204A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 200L, * 30kW (50 Hz) 33.5kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",3358,"ΤΕΜ",1,"LVM",1,"1LE15012AA433JB6"]
["1LE1501-2AA52-2FA5","SIMOTICS SD MOTOR TYPE: 1CV2205A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 200L, * 37kW (50 Hz) 41.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF350 (A400) without motor protection Terminal box on RHS",3874,"ΤΕΜ",1,"LVM",1,"1LE15012AA522FA5"]
["1LE1501-2AA53-4FA4","SIMOTICS SD MOTOR TYPE: 1CV2205A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 200L, * 37kW (50 Hz) 41.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF350 (A400) without motor protection Terminal box at top",3691,"ΤΕΜ",1,"LVM",1,"1LE15012AA534FA4"]
["1LE1501-2AB52-2FC5","SIMOTICS SD MOTOR TYPE: 1CV2205B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 200L, * 30kW (50 Hz) 34.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF350 (A400) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",3287,"ΤΕΜ",1,"LVM",1,"1LE15012AB522FC5"]
["1LE1501-2AB53-3GA5","SIMOTICS SD MOTOR TYPE: 1CV2205B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 200L, * 30kW (50 Hz) 34.5kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF350 (A400) without motor protection Terminal box on RHS",3176,"ΤΕΜ",1,"LVM",1,"1LE15012AB533GA5"]
["1LE1501-2AC42-2JA6","SIMOTICS SD MOTOR TYPE: 1CV2204C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 200L, * 18.5 kW (50 Hz) 22 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF350 (A400) without motor protection Terminal box on left-hand side",3166,"ΤΕΜ",1,"LVM",1,"1LE15012AC422JA6"]
["1LE1501-2AC50-4FB4","SIMOTICS SD MOTOR TYPE: 1CV2205C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 200L, * 22kW (50 Hz) 26.5kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",3489,"ΤΕΜ",1,"LVM",1,"1LE15012AC504FB4"]
["1LE1501-2AC52-2WC4","SIMOTICS SD MOTOR TYPE: 1CV2205C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 200L, * 22kW (50 Hz) 26.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 15 * Flange: FF350 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",3629,"ΤΕΜ",1,"LVM",1,"1LE15012AC522WC4"]
["1LE1501-2AC53-3JA4","SIMOTICS SD MOTOR TYPE: 1CV2205C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 200L, * 22kW (50 Hz) 26.5kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF350 (A400) without motor protection Terminal box at top",3494,"ΤΕΜ",1,"LVM",1,"1LE15012AC533JA4"]
["1LE1501-2BA22-1JA6","SIMOTICS SD MOTOR TYPE: 1CV2222A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 225M * 45kW (50 Hz) 51kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF400 (A450) without motor protection Terminal box on left-hand side",4628,"ΤΕΜ",1,"LVM",1,"1LE15012BA221JA6"]
["1LE1501-2BA23-3WB6","SIMOTICS SD MOTOR TYPE: 1CV2222A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 225M * 45kW (50 Hz) 51kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 15 * Flange: FF400 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",4840,"ΤΕΜ",1,"LVM",1,"1LE15012BA233WB6"]
["1LE1501-2BB00-4WB5","SIMOTICS SD MOTOR TYPE: 1CV2220B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 225S * 37kW (50 Hz) 42.5kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF400 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",3922,"ΤΕΜ",1,"LVM",1,"1LE15012BB004WB5"]
["1LE1501-2BB03-4FA6","SIMOTICS SD MOTOR TYPE: 1CV2220B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 225S * 37kW (50 Hz) 42.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF400 (A450) without motor protection Terminal box on left-hand side",3667,"ΤΕΜ",1,"LVM",1,"1LE15012BB034FA6"]
["1LE1501-2BB22-2JA4","SIMOTICS SD MOTOR TYPE: 1CV2222B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 225M * 45kW (50 Hz) 52kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF400 (A450) without motor protection Terminal box at top",4077,"ΤΕΜ",1,"LVM",1,"1LE15012BB222JA4"]
["1LE1501-2BB23-4GA6","SIMOTICS SD MOTOR TYPE: 1CV2222B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 225M * 45kW (50 Hz) 52kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF400 (A450) without motor protection Terminal box on left-hand side",4251,"ΤΕΜ",1,"LVM",1,"1LE15012BB234GA6"]
["1LE1501-2BC22-2GC5","SIMOTICS SD MOTOR TYPE: 1CV2222C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 225M * 30kW (50 Hz) 36 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF400 (A450) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",4826,"ΤΕΜ",1,"LVM",1,"1LE15012BC222GC5"]
["1LE1501-2BC23-4AA4","SIMOTICS SD MOTOR TYPE: 1CV2222C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 225M * 30kW (50 Hz) 36 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box at top",4200,"ΤΕΜ",1,"LVM",1,"1LE15012BC234AA4"]
["1LE1501-2CA22-2JC4","SIMOTICS SD MOTOR TYPE: 1CV2252A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 250M * 55kW (50 Hz) 62kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF500 (A550) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",5369,"ΤΕΜ",1,"LVM",1,"1LE15012CA222JC4"]
["1LE1501-2CB20-4GA6","SIMOTICS SD MOTOR TYPE: 1CV2252B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 250M * 55kW (50 Hz) 63kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF500 (A550) without motor protection Terminal box on left-hand side",5202,"ΤΕΜ",1,"LVM",1,"1LE15012CB204GA6"]
["1LE1501-2CB22-1JB4","SIMOTICS SD MOTOR TYPE: 1CV2252B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 250M * 55kW (50 Hz) 63kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",5211,"ΤΕΜ",1,"LVM",1,"1LE15012CB221JB4"]
["1LE1501-2CB23-3JB5","SIMOTICS SD MOTOR TYPE: 1CV2252B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 250M * 55kW (50 Hz) 63kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",5534,"ΤΕΜ",1,"LVM",1,"1LE15012CB233JB5"]
["1LE1501-2CC22-2AB4","SIMOTICS SD MOTOR TYPE: 1CV2252C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 250M * 37kW (50 Hz) 44.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",5219,"ΤΕΜ",1,"LVM",1,"1LE15012CC222AB4"]
["1LE1501-2CC23-4AB5","SIMOTICS SD MOTOR TYPE: 1CV2252C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 250M * 37kW (50 Hz) 44.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",5542,"ΤΕΜ",1,"LVM",1,"1LE15012CC234AB5"]
["1LE1501-2DA02-1AA6","SIMOTICS SD MOTOR TYPE: 1CV2280A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 280S, * 75kW (50 Hz) 84kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, without motor protection Terminal box on left-hand side",7174,"ΤΕΜ",1,"LVM",1,"1LE15012DA021AA6"]
["1LE1501-2DA20-4AB5","SIMOTICS SD MOTOR TYPE: 1CV2282A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 280M * 90kW (50 Hz) 101kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",8429,"ΤΕΜ",1,"LVM",1,"1LE15012DA204AB5"]
["1LE1501-2DA23-3AA5","SIMOTICS SD MOTOR TYPE: 1CV2282A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 280M * 90kW (50 Hz) 101kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, without motor protection Terminal box on RHS",8392,"ΤΕΜ",1,"LVM",1,"1LE15012DA233AA5"]
["1LE1501-2DB02-1GA6","SIMOTICS SD MOTOR TYPE: 1CV2280B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 280S, * 75kW (50 Hz) 86kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF500 (A550) without motor protection Terminal box on left-hand side",7066,"ΤΕΜ",1,"LVM",1,"1LE15012DB021GA6"]
["1LE1501-2DB02-2AC6","SIMOTICS SD MOTOR TYPE: 1CV2280B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 280S, * 75kW (50 Hz) 86kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",6906,"ΤΕΜ",1,"LVM",1,"1LE15012DB022AC6"]
["1LE1501-2DB20-4AA5","SIMOTICS SD MOTOR TYPE: 1CV2282B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 280M * 90kW (50 Hz) 104kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box on RHS",7713,"ΤΕΜ",1,"LVM",1,"1LE15012DB204AA5"]
["1LE1501-2DB22-2JB6","SIMOTICS SD MOTOR TYPE: 1CV2282B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 280M * 90kW (50 Hz) 104kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",8281,"ΤΕΜ",1,"LVM",1,"1LE15012DB222JB6"]
["1LE1501-2DB23-4JB5","SIMOTICS SD MOTOR TYPE: 1CV2282B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 280M * 90kW (50 Hz) 104kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",8281,"ΤΕΜ",1,"LVM",1,"1LE15012DB234JB5"]
["1LE1501-2DC03-3GA6","SIMOTICS SD MOTOR TYPE: 1CV2280C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 280S, * 45kW (50 Hz) 54kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF500 (A550) without motor protection Terminal box on left-hand side",7024,"ΤΕΜ",1,"LVM",1,"1LE15012DC033GA6"]
["1LE1501-2DC22-1WB6","SIMOTICS SD MOTOR TYPE: 1CV2282C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 280M * 55kW (50 Hz) 66kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 15 * Flange: FF500 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",8542,"ΤΕΜ",1,"LVM",1,"1LE15012DC221WB6"]
["1LE1501-2DC23-3JB5","SIMOTICS SD MOTOR TYPE: 1CV2282C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 280M * 55kW (50 Hz) 66kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",8414,"ΤΕΜ",1,"LVM",1,"1LE15012DC233JB5"]
["1LE1501-3AA02-2AC5","SIMOTICS SD MOTOR TYPE: 1CV2310A low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 315S, * 110kW (50 Hz) 123kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",10111,"ΤΕΜ",1,"LVM",1,"1LE15013AA022AC5"]
["1LE1501-3AA03-3FA5","SIMOTICS SD MOTOR TYPE: 1CV2310A low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 315S, * 110kW (50 Hz) 123kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 5, Flange: FF600 (A660) without motor protection Terminal box on RHS",10440,"ΤΕΜ",1,"LVM",1,"1LE15013AA033FA5"]
["1LE1501-3AA23-3GA4","SIMOTICS SD MOTOR TYPE: 1CV2312A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 315M, * 132kW (50 Hz) 148kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, Flange: FF600 (A660) without motor protection Terminal box at top",11959,"ΤΕΜ",1,"LVM",1,"1LE15013AA233GA4"]
["1LE1501-3AA23-3GB5","SIMOTICS SD MOTOR TYPE: 1CV2312A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 315M, * 132kW (50 Hz) 148kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",12546,"ΤΕΜ",1,"LVM",1,"1LE15013AA233GB5"]
["1LE1501-3AA42-2GA6","SIMOTICS SD MOTOR TYPE: 1CV2314A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 315L, * 160kW (50 Hz) 180kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, Flange: FF600 (A660) without motor protection Terminal box on left-hand side",15160,"ΤΕΜ",1,"LVM",1,"1LE15013AA422GA6"]
["1LE1501-3AA52-2AB6","SIMOTICS SD MOTOR TYPE: 1CV2315A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 315L, * 200kW (50 Hz) 224kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",18144,"ΤΕΜ",1,"LVM",1,"1LE15013AA522AB6"]
["1LE1501-3AB02-1FA6","SIMOTICS SD MOTOR TYPE: 1CV2310B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 315S, * 110kW (50 Hz) 127kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, Flange: FF600 (A660) without motor protection Terminal box on left-hand side",10230,"ΤΕΜ",1,"LVM",1,"1LE15013AB021FA6"]
["1LE1501-3AB03-3JB5","SIMOTICS SD MOTOR TYPE: 1CV2310B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 315S, * 110kW (50 Hz) 127kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",10463,"ΤΕΜ",1,"LVM",1,"1LE15013AB033JB5"]
["1LE1501-3AB22-1AB4","SIMOTICS SD MOTOR TYPE: 1CV2312B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 315M, * 132kW (50 Hz) 152kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",11264,"ΤΕΜ",1,"LVM",1,"1LE15013AB221AB4"]
["1LE1501-3AB23-4JB5","SIMOTICS SD MOTOR TYPE: 1CV2312B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 315M, * 132kW (50 Hz) 152kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",12012,"ΤΕΜ",1,"LVM",1,"1LE15013AB234JB5"]
["1LE1501-3AB43-4JC5","SIMOTICS SD MOTOR TYPE: 1CV2314B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 315L, * 160kW (50 Hz) 184kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF600 (A660) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",14353,"ΤΕΜ",1,"LVM",1,"1LE15013AB434JC5"]
["1LE1501-3AB50-4JA5","SIMOTICS SD MOTOR TYPE: 1CV2315B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 315L, * 200kW (50 Hz) 230kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF600 (A660) without motor protection Terminal box on RHS",17386,"ΤΕΜ",1,"LVM",1,"1LE15013AB504JA5"]
["1LE1501-3AC02-2FA5","SIMOTICS SD MOTOR TYPE: 1CV2310C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 315S, * 75kW (50 Hz) 90 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, Flange: FF600 (A660) without motor protection Terminal box on RHS",10939,"ΤΕΜ",1,"LVM",1,"1LE15013AC022FA5"]
["1LE1501-3AC03-3GB4","SIMOTICS SD MOTOR TYPE: 1CV2310C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 315S, * 75kW (50 Hz) 90 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",10869,"ΤΕΜ",1,"LVM",1,"1LE15013AC033GB4"]
["1LE1501-3AC22-1GA6","SIMOTICS SD MOTOR TYPE: 1CV2312C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 315M, * 90kW (50 Hz) 108kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, Flange: FF600 (A660) without motor protection Terminal box on left-hand side",12376,"ΤΕΜ",1,"LVM",1,"1LE15013AC221GA6"]
["1LE1501-3AC23-3FA6","SIMOTICS SD MOTOR TYPE: 1CV2312C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 315M, * 90kW (50 Hz) 108kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 5, Flange: FF600 (A660) without motor protection Terminal box on left-hand side",12372,"ΤΕΜ",1,"LVM",1,"1LE15013AC233FA6"]
["1LE1501-3AC43-3AB5","SIMOTICS SD MOTOR TYPE: 1CV2314C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 315L, * 110kW (50 Hz) 132 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",14369,"ΤΕΜ",1,"LVM",1,"1LE15013AC433AB5"]
["1LE1501-3AC52-1GB6","SIMOTICS SD MOTOR TYPE: 1CV2315C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations to be considered! 6-pole * Size 315L, * 132kW (50 Hz) 158kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",17460,"ΤΕΜ",1,"LVM",1,"1LE15013AC521GB6"]
["1LE1501-3AC63-3JB4","SIMOTICS SD MOTOR TYPE: 1CV2316C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations to be considered! 6-pole * Size 315L, * 160kW (50 Hz) 192kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",20504,"ΤΕΜ",1,"LVM",1,"1LE15013AC633JB4"]
["1LE1503-0CA22-1AA4","SIMOTICS SD MOTOR TYPE: 1CV3072A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 71M * 0.37kW (50 Hz) 0.43kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, without motor protection Terminal box at top",297,"ΤΕΜ",1,"LVM",1,"1LE15030CA221AA4"]
["1LE1503-0DA20-4JB4","SIMOTICS SD MOTOR TYPE: 1CV3082A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 80M * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF165 (A200) 1 PTC thermistor for disconnection (2 terminals) Terminal box at top",383,"ΤΕΜ",1,"LVM",1,"1LE15030DA204JB4"]
["1LE1503-0DA23-3JA4","SIMOTICS SD MOTOR TYPE: 1CV3082A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 80M * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 35 * Flange: FF165 (A200) without motor protection Terminal box at top",382,"ΤΕΜ",1,"LVM",1,"1LE15030DA233JA4"]
["1LE1503-0DA32-2AC6","SIMOTICS SD MOTOR TYPE: 1CV3083A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 80M * 1.1kW (50 Hz) 1.27kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 2 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",486,"ΤΕΜ",1,"LVM",1,"1LE15030DA322AC6"]
["1LE1503-0EA02-1JA4","SIMOTICS SD MOTOR TYPE: 1CV3090A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 90S * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF165 (A200) without motor protection Terminal box at top",497,"ΤΕΜ",1,"LVM",1,"1LE15030EA021JA4"]
["1LE1503-0EA42-1GA4","SIMOTICS SD MOTOR TYPE: 1CV3094A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 90L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF165 (A200) without motor protection Terminal box at top",601,"ΤΕΜ",1,"LVM",1,"1LE15030EA421GA4"]
["1LE1503-1AA40-4AB5","SIMOTICS SD MOTOR TYPE: 1CV3104A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",640,"ΤΕΜ",1,"LVM",1,"1LE15031AA404AB5"]
["1LE1503-1AA43-3AA7","SIMOTICS SD MOTOR TYPE: 1CV3104A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, without motor protection Terminal box below",613,"ΤΕΜ",1,"LVM",1,"1LE15031AA433AA7"]
["1LE1503-1AC42-2FA4","SIMOTICS SD MOTOR TYPE: 1CV3104C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 100L * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF215 (A250) without motor protection Terminal box at top",518,"ΤΕΜ",1,"LVM",1,"1LE15031AC422FA4"]
["1LE1503-1BA23-4AB5","SIMOTICS SD MOTOR TYPE: 1CV3112A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",741,"ΤΕΜ",1,"LVM",1,"1LE15031BA234AB5"]
["1LE1503-1BA23-4JA6","SIMOTICS SD MOTOR TYPE: 1CV3112A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF215 (A250) without motor protection Terminal box on left-hand side",737,"ΤΕΜ",1,"LVM",1,"1LE15031BA234JA6"]
["1LE1503-1CA03-4JA6","SIMOTICS SD MOTOR TYPE: 1CV3130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF265 (A300) without motor protection Terminal box on left-hand side",912,"ΤΕΜ",1,"LVM",1,"1LE15031CA034JA6"]
["1LE1503-1CA10-4GB5","SIMOTICS SD MOTOR TYPE: 1CV3131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",1212,"ΤΕΜ",1,"LVM",1,"1LE15031CA104GB5"]
["1LE1001-0BA22-2GA4","SIMOTICS GP Motor type: 1AV2062A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 63M * 0.18kW (50 Hz) 0.21kW(60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, Flange: FF115 (A140) without motor protection Terminal box at top",195,"ΤΕΜ",1,"LVM",1,"1LE10010BA222GA4"]
["1LE1001-0BA33-4AB4","SIMOTICS GP Motor type: 1AV2063A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 63M * 0.25 kW (50 Hz) 0.29kW(60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 1 PTC thermistor for disconnection (2 terminals) Terminal box at top",202,"ΤΕΜ",1,"LVM",1,"1LE10010BA334AB4"]
["1LE1001-0CA33-4AC4","SIMOTICS GP Motor type: 1AV2073A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 71M * 0.55 kW (50 Hz) 0.63kW(60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 2 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",287,"ΤΕΜ",1,"LVM",1,"1LE10010CA334AC4"]
["1LE1001-0DA22-2JA6","SIMOTICS GP Motor type: 1AV2082A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 80M * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF165 (A200) without motor protection Terminal box lateral left",260,"ΤΕΜ",1,"LVM",1,"1LE10010DA222JA6"]
["1LE1001-0DA32-1FB5","SIMOTICS GP Motor type: 1AV2083A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 80M * 1.1kW (50 Hz) 1.27kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF165 (A200) 1 PTC thermistor for disconnection (2 terminals) Terminal box lateral right",322,"ΤΕΜ",1,"LVM",1,"1LE10010DA321FB5"]
["1LE1001-0DA33-4GC4","SIMOTICS GP Motor type: 1AV2083A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 80M * 1.1kW (50 Hz) 1.27kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF165 (A200) 2 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",350,"ΤΕΜ",1,"LVM",1,"1LE10010DA334GC4"]
["1LE1001-0DB22-2GB4","SIMOTICS GP Motor type: 1AV2082B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency 4-pole * Size 80M * 0.55kW (50 Hz) 60Hz: IEC 60034-30 0.63kW 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF165 (A200) 1 PTC thermistor for disconnection (2 terminals) Terminal box at top",258,"ΤΕΜ",1,"LVM",1,"1LE10010DB222GB4"]
["1LE1001-0DB23-4GB4","SIMOTICS GP Motor type: 1AV2082B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency 4-pole * Size 80M * 0.55kW (50 Hz) 60Hz: IEC 60034-30 0.63kW 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF165 (A200) 1 PTC thermistor for disconnection (2 terminals) Terminal box at top",258,"ΤΕΜ",1,"LVM",1,"1LE10010DB234GB4"]
["1LE1001-0DB32-2AA6","SIMOTICS GP Motor type: 1AV2083B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 80M * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, without motor protection Terminal box lateral left",254,"ΤΕΜ",1,"LVM",1,"1LE10010DB322AA6"]
["1LE1001-0DB33-4FC6","SIMOTICS GP Motor type: 1AV2083B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 80M * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF165 (A200) 2 PTC thermistors for warning and shutdown (4 terminals) Terminal box lateral left",351,"ΤΕΜ",1,"LVM",1,"1LE10010DB334FC6"]
["1LE1001-0EA02-2JC5","SIMOTICS GP Motor type: 1AV2090A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 90S * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF165 (A200) 2 PTC thermistors for warning and shutdown (4 terminals) Terminal box lateral right",411,"ΤΕΜ",1,"LVM",1,"1LE10010EA022JC5"]
["1LE1001-0EA40-4FA6","SIMOTICS GP Motor type: 1AV2094A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 90L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF165 (A200) without motor protection Terminal box lateral left",421,"ΤΕΜ",1,"LVM",1,"1LE10010EA404FA6"]
["1LE1001-0EA43-4GB5","SIMOTICS GP Motor type: 1AV2094A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 90L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF165 (A200) 1 PTC thermistor for disconnection (2 terminals) Terminal box lateral right",439,"ΤΕΜ",1,"LVM",1,"1LE10010EA434GB5"]
["1LE1001-0EB02-2GC6","SIMOTICS GP Motor type: 1AV2090B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 90S * 1.1kW (50 Hz) 1.27kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF165 (A200) 2 PTC thermistors for warning and shutdown (4 terminals) Terminal box lateral left",401,"ΤΕΜ",1,"LVM",1,"1LE10010EB022GC6"]
["1LE1001-0EB03-4FC6","SIMOTICS GP Motor type: 1AV2090B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 90S * 1.1kW (50 Hz) 1.27kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF165 (A200) 2 PTC thermistors for warning and shutdown (4 terminals) Terminal box lateral left",401,"ΤΕΜ",1,"LVM",1,"1LE10010EB034FC6"]
["1LE1001-0EB43-3JB5","SIMOTICS GP Motor type: 1AV2094B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 90L * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 35 * Flange: FF165 (A200) 1 PTC thermistor for disconnection (2 terminals) Terminal box lateral right",418,"ΤΕΜ",1,"LVM",1,"1LE10010EB433JB5"]
["1LE1001-0EB43-4GA5","SIMOTICS GP Motor type: 1AV2094B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 90L * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF165 (A200) without motor protection Terminal box lateral right",380,"ΤΕΜ",1,"LVM",1,"1LE10010EB434GA5"]
["1LE1001-0EC03-4GC5","SIMOTICS GP Motor type: 1AV2090C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 90S * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF165 (A200) 2 PTC thermistors for warning and shutdown (4 terminals) Terminal box lateral right",396,"ΤΕΜ",1,"LVM",1,"1LE10010EC034GC5"]
["1LE1001-0EC40-4GB5","SIMOTICS GP Motor type: 1AV2094C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 60 Hz, P60: IE1 6-pole * Size 90L * 1.10kW (50 Hz) 1.27kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF165 (A200) 1 PTC thermistor for disconnection (2 terminals) Terminal box lateral right",407,"ΤΕΜ",1,"LVM",1,"1LE10010EC404GB5"]
["1LE1001-0EC43-4GB4","SIMOTICS GP Motor type: 1AV2094C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 60 Hz, P60: IE1 6-pole * Size 90L * 1.10kW (50 Hz) 1.27kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF165 (A200) 1 PTC thermistor for disconnection (2 terminals) Terminal box at top",390,"ΤΕΜ",1,"LVM",1,"1LE10010EC434GB4"]
["1LE1001-1AA42-1GA4","SIMOTICS GP Motor type: 1AV2104A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 kW (60Hz), 50 Hz power 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF215 (A250) without motor protection Terminal box at top",498,"ΤΕΜ",1,"LVM",1,"1LE10011AA421GA4"]
["1LE1001-1AA43-3GA6","SIMOTICS GP Motor type: 1AV2104A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 kW (60Hz), 50 Hz power 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF215 (A250) without motor protection Terminal box on left-hand side",542,"ΤΕΜ",1,"LVM",1,"1LE10011AA433GA6"]
["1LE1001-1AB42-1AB4","SIMOTICS GP Motor type: 1AV2104B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 100L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",476,"ΤΕΜ",1,"LVM",1,"1LE10011AB421AB4"]
["1LE1001-1AB43-3JB6","SIMOTICS GP Motor type: 1AV2104B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 100L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 35 * Flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",557,"ΤΕΜ",1,"LVM",1,"1LE10011AB433JB6"]
["1LE1001-1AB52-1FA6","SIMOTICS GP Motor type: 1AV2105B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF215 (A250) without motor protection Terminal box on left-hand side",563,"ΤΕΜ",1,"LVM",1,"1LE10011AB521FA6"]
["1LE1001-1AB53-3GA7","SIMOTICS GP Motor type: 1AV2105B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF215 (A250) without motor protection Terminal box below",563,"ΤΕΜ",1,"LVM",1,"1LE10011AB533GA7"]
["1LE1001-1AB53-4JC7","SIMOTICS GP Motor type: 1AV2105B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF215 (A250) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",630,"ΤΕΜ",1,"LVM",1,"1LE10011AB534JC7"]
["1LE1001-1AC42-1AA7","SIMOTICS GP Motor type: 1AV2104C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 100L * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, without motor protection Terminal box below",465,"ΤΕΜ",1,"LVM",1,"1LE10011AC421AA7"]
["1LE1001-1AC43-3JB4","SIMOTICS GP Motor type: 1AV2104C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 100L * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 35 * Flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",509,"ΤΕΜ",1,"LVM",1,"1LE10011AC433JB4"]
["1LE1001-1BA20-4GA5","SIMOTICS GP Motor type: 1AV2112A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF215 (A250) without motor protection Terminal box on RHS",615,"ΤΕΜ",1,"LVM",1,"1LE10011BA204GA5"]
["1LE1001-1BA23-3FB5","SIMOTICS GP Motor type: 1AV2112A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 5, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",693,"ΤΕΜ",1,"LVM",1,"1LE10011BA233FB5"]
["1LE1001-1BB22-1GB4","SIMOTICS GP Motor type: 1AV2112B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",692,"ΤΕΜ",1,"LVM",1,"1LE10011BB221GB4"]
["1LE1001-1BB23-3AA6","SIMOTICS GP Motor type: 1AV2112B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 3, without motor protection Terminal box on left-hand side",647,"ΤΕΜ",1,"LVM",1,"1LE10011BB233AA6"]
["1LE1001-1BC20-4AB4","SIMOTICS GP Motor type: 1AV2112C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 112M, * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",550,"ΤΕΜ",1,"LVM",1,"1LE10011BC204AB4"]
["1LE1001-1BC22-1GA5","SIMOTICS GP Motor type: 1AV2112C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 112M, * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF215 (A250) without motor protection Terminal box on RHS",618,"ΤΕΜ",1,"LVM",1,"1LE10011BC221GA5"]
["1LE1001-1CA00-4FA6","SIMOTICS GP Motor type: 1AV2130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF265 (A300) without motor protection Terminal box on left-hand side",763,"ΤΕΜ",1,"LVM",1,"1LE10011CA004FA6"]
["1LE1001-1CA00-4GB5","SIMOTICS GP Motor type: 1AV2130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",838,"ΤΕΜ",1,"LVM",1,"1LE10011CA004GB5"]
["1LE1001-1CA02-2GC6","SIMOTICS GP Motor type: 1AV2130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",878,"ΤΕΜ",1,"LVM",1,"1LE10011CA022GC6"]
["1LE1001-1CA10-4JA7","SIMOTICS GP Motor type: 1AV2131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF265 (A300) without motor protection Terminal box below",941,"ΤΕΜ",1,"LVM",1,"1LE10011CA104JA7"]
["1LE1001-1CA12-2GA6","SIMOTICS GP Motor type: 1AV2131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF265 (A300) without motor protection Terminal box on left-hand side",939,"ΤΕΜ",1,"LVM",1,"1LE10011CA122GA6"]
["1LE1001-1CA13-4AB6","SIMOTICS GP Motor type: 1AV2131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",959,"ΤΕΜ",1,"LVM",1,"1LE10011CA134AB6"]
["1LE1001-1CB00-4GB6","SIMOTICS GP Motor type: 1AV2130B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",889,"ΤΕΜ",1,"LVM",1,"1LE10011CB004GB6"]
["1LE1001-1CB03-3WB5","SIMOTICS GP Motor type: 1AV2130B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 15 * Flange: FF265 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",938,"ΤΕΜ",1,"LVM",1,"1LE10011CB033WB5"]
["1LE1001-1CB03-3WB7","SIMOTICS GP Motor type: 1AV2130B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 15 * Flange: FF265 3 PTC thermistors for disconnection (2 terminals) Terminal box below",938,"ΤΕΜ",1,"LVM",1,"1LE10011CB033WB7"]
["1LE1001-1CB22-1AA5","SIMOTICS GP Motor type: 1AV2132B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations to be considered! 4-pole * Size 132M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, without motor protection Terminal box on RHS",986,"ΤΕΜ",1,"LVM",1,"1LE10011CB221AA5"]
["1LE1001-1CB23-4AC4","SIMOTICS GP Motor type: 1AV2132B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations to be considered! 4-pole * Size 132M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",1014,"ΤΕΜ",1,"LVM",1,"1LE10011CB234AC4"]
["1LE1001-1CB23-4WC7","SIMOTICS GP Motor type: 1AV2132B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations to be considered! 4-pole * Size 132M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF265 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",1136,"ΤΕΜ",1,"LVM",1,"1LE10011CB234WC7"]
["1LE1001-1CC02-2GC4","SIMOTICS GP Motor type: 1AV2130C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 132S, * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",805,"ΤΕΜ",1,"LVM",1,"1LE10011CC022GC4"]
["1LE1001-1CC03-3AA5","SIMOTICS GP Motor type: 1AV2130C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 132S, * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 3, without motor protection Terminal box on RHS",722,"ΤΕΜ",1,"LVM",1,"1LE10011CC033AA5"]
["1LE1001-1CC20-4JA4","SIMOTICS GP Motor type: 1AV2132C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 132M, * 4kW (50 Hz) 4.6 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF265 (A300) without motor protection Terminal box at top",839,"ΤΕΜ",1,"LVM",1,"1LE10011CC204JA4"]
["1LE1001-1CC23-3FA5","SIMOTICS GP Motor type: 1AV2132C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 132M, * 4kW (50 Hz) 4.6 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 5, flange: FF265 (A300) without motor protection Terminal box on RHS",924,"ΤΕΜ",1,"LVM",1,"1LE10011CC233FA5"]
["1LE1001-1CC23-4JA7","SIMOTICS GP Motor type: 1AV2132C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 132M, * 4kW (50 Hz) 4.6 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF265 (A300) without motor protection Terminal box below",891,"ΤΕΜ",1,"LVM",1,"1LE10011CC234JA7"]
["1LE1001-1CC32-2FA6","SIMOTICS GP Motor type: 1AV2133C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 132M, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF265 (A300) without motor protection Terminal box on left-hand side",1095,"ΤΕΜ",1,"LVM",1,"1LE10011CC322FA6"]
["1LE1001-1CC32-2WC5","SIMOTICS GP Motor type: 1AV2133C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 132M, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 15 * Flange: FF265 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",1224,"ΤΕΜ",1,"LVM",1,"1LE10011CC322WC5"]
["1LE1001-1CC33-4FB6","SIMOTICS GP Motor type: 1AV2133C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 132M, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1170,"ΤΕΜ",1,"LVM",1,"1LE10011CC334FB6"]
["1LE1001-1DA22-1FB6","SIMOTICS GP Motor type: 1AV2162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1401,"ΤΕΜ",1,"LVM",1,"1LE10011DA221FB6"]
["1LE1001-1DA23-3AB7","SIMOTICS GP Motor type: 1AV2162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1330,"ΤΕΜ",1,"LVM",1,"1LE10011DA233AB7"]
["1LE1001-1DA32-1GA5","SIMOTICS GP Motor type: 1AV2163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF300 (A350) without motor protection Terminal box on RHS",1678,"ΤΕΜ",1,"LVM",1,"1LE10011DA321GA5"]
["1LE1001-1DA32-2FC4","SIMOTICS GP Motor type: 1AV2163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",1695,"ΤΕΜ",1,"LVM",1,"1LE10011DA322FC4"]
["1LE1001-1DA33-4GC6","SIMOTICS GP Motor type: 1AV2163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",1750,"ΤΕΜ",1,"LVM",1,"1LE10011DA334GC6"]
["1LE1001-1DA42-1FA4","SIMOTICS GP Motor type: 1AV2164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations to be considered! 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",1913,"ΤΕΜ",1,"LVM",1,"1LE10011DA421FA4"]
["1LE1001-1DA43-3GB7","SIMOTICS GP Motor type: 1AV2164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations to be considered! 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",2044,"ΤΕΜ",1,"LVM",1,"1LE10011DA433GB7"]
["1LE1001-1DA43-4FC5","SIMOTICS GP Motor type: 1AV2164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations to be considered! 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",2040,"ΤΕΜ",1,"LVM",1,"1LE10011DA434FC5"]
["1LE1001-1DB22-1GB5","SIMOTICS GP Motor type: 1AV2162B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",1431,"ΤΕΜ",1,"LVM",1,"1LE10011DB221GB5"]
["1LE1001-1DB23-4GA6","SIMOTICS GP Motor type: 1AV2162B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) without motor protection Terminal box on left-hand side",1312,"ΤΕΜ",1,"LVM",1,"1LE10011DB234GA6"]
["1LE1001-1DB40-4GA7","SIMOTICS GP Motor type: 1AV2164B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 160L, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) without motor protection Terminal box below",1652,"ΤΕΜ",1,"LVM",1,"1LE10011DB404GA7"]
["1LE1001-1DB42-2FC5","SIMOTICS GP Motor type: 1AV2164B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 160L, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",1767,"ΤΕΜ",1,"LVM",1,"1LE10011DB422FC5"]
["1LE1001-1DB43-4FC6","SIMOTICS GP Motor type: 1AV2164B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 160L, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",1767,"ΤΕΜ",1,"LVM",1,"1LE10011DB434FC6"]
["1LE1001-1DC22-2AC6","SIMOTICS GP Motor type: 1AV2162C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 6-pole * Size 160M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",1414,"ΤΕΜ",1,"LVM",1,"1LE10011DC222AC6"]
["1LE1001-1DC22-2GB7","SIMOTICS GP Motor type: 1AV2162C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 6-pole * Size 160M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1446,"ΤΕΜ",1,"LVM",1,"1LE10011DC222GB7"]
["1LE1001-1DC42-1AA6","SIMOTICS GP Motor type: 1AV2164C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 6-pole * Size 160L, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, without motor protection Terminal box on left-hand side",1817,"ΤΕΜ",1,"LVM",1,"1LE10011DC421AA6"]
["1LE1001-1DC42-1GB7","SIMOTICS GP Motor type: 1AV2164C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 6-pole * Size 160L, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1964,"ΤΕΜ",1,"LVM",1,"1LE10011DC421GB7"]
["1LE1001-1DC43-4FA6","SIMOTICS GP Motor type: 1AV2164C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 6-pole * Size 160L, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF300 (A350) without motor protection Terminal box on left-hand side",1845,"ΤΕΜ",1,"LVM",1,"1LE10011DC434FA6"]
["1LE1002-0BA22-2JA4","SIMOTICS GP Motor type: 1AV1062A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) aluminum housing Standard efficiency IE1, 2-pole * Size 63M * 0.18kW (50 Hz) 0.21kW(60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF115 (A140) Without motor protection Terminal box at top",155,"ΤΕΜ",1,"LVM",1,"1LE10020BA222JA4"]
["1LE1002-0CA23-3GB4","SIMOTICS GP Motor type: 1AV1072A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) aluminum housing Standard efficiency IE1, 2-pole * Size 71M * 0.37 kW (50 Hz) 0.43kW(60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF130 (A160) 1 PTC thermistor for disconnection (2 terminals) Terminal box at top",195,"ΤΕΜ",1,"LVM",1,"1LE10020CA233GB4"]
["1LE1003-0DA22-1FB6","SIMOTICS GP MOTOR TYPE: 1AV3082A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 80M * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF165 (A200) MOTOR PROTECTION WITH 1 PTC THERMISTORS FOR SHUTDOWN Terminal box lateral left",334,"ΤΕΜ",1,"LVM",1,"1LE10030DA221FB6"]
["1LE1003-0DA32-1AA5","SIMOTICS GP MOTOR TYPE: 1AV3083A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 80M * 1.1kW (50 Hz) 1.27kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, WITHOUT MOTOR PROTECTION Terminal box lateral right",334,"ΤΕΜ",1,"LVM",1,"1LE10030DA321AA5"]
["1LE1003-0DA32-2GC4","SIMOTICS GP MOTOR TYPE: 1AV3083A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 80M * 1.1kW (50 Hz) 1.27kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF165 (A200) 2 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",400,"ΤΕΜ",1,"LVM",1,"1LE10030DA322GC4"]
["1LE1003-0DB22-1AB6","SIMOTICS GP MOTOR TYPE: 1AV3082B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing Premium Efficiency, 4-pole * Size 80M * 0.55kW (50 Hz) 0.63kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, MOTOR PROTECTION WITH 1 PTC THERMISTORS FOR SHUTDOWN Terminal box lateral left",308,"ΤΕΜ",1,"LVM",1,"1LE10030DB221AB6"]
["1LE1003-0DB23-3AB6","SIMOTICS GP MOTOR TYPE: 1AV3082B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing Premium Efficiency, 4-pole * Size 80M * 0.55kW (50 Hz) 0.63kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 3, MOTOR PROTECTION WITH 1 PTC THERMISTORS FOR SHUTDOWN Terminal box lateral left",308,"ΤΕΜ",1,"LVM",1,"1LE10030DB233AB6"]
["1LE1003-0DB32-2FC5","SIMOTICS GP MOTOR TYPE: 1AV3083B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 80M * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF165 (A200) 2 PTC thermistors for warning and shutdown (4 terminals) Terminal box lateral right",399,"ΤΕΜ",1,"LVM",1,"1LE10030DB322FC5"]
["1LE1003-0DB33-3AB5","SIMOTICS GP MOTOR TYPE: 1AV3083B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 80M * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 3, MOTOR PROTECTION WITH 1 PTC THERMISTORS FOR SHUTDOWN Terminal box lateral right",332,"ΤΕΜ",1,"LVM",1,"1LE10030DB333AB5"]
["1LE1003-0DC20-4GB5","SIMOTICS GP MOTOR TYPE: 1AV3082C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing Premium Efficiency, 6-pole * Size 80M * 0.37kW (50 Hz) 0.43kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF165 (A200) 1 PTC thermistor for disconnection (2 terminals) Terminal box lateral right",309,"ΤΕΜ",1,"LVM",1,"1LE10030DC204GB5"]
["1LE1003-0DC30-4GA4","SIMOTICS GP MOTOR TYPE: 1AV3083C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing Premium Efficiency, 6-pole * Size 80M * 0.55kW (50 Hz) 0.63kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF165 (A200) without motor protection Terminal box at top",318,"ΤΕΜ",1,"LVM",1,"1LE10030DC304GA4"]
["1LE1003-0EA00-4JA6","SIMOTICS GP MOTOR TYPE: 1AV3090A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 90S * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF165 (A200) WITHOUT MOTOR PROTECTION Terminal box lateral left",396,"ΤΕΜ",1,"LVM",1,"1LE10030EA004JA6"]
["1LE1003-0EA02-2JA5","SIMOTICS GP MOTOR TYPE: 1AV3090A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 90S * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF165 (A200) WITHOUT MOTOR PROTECTION Terminal box lateral right",396,"ΤΕΜ",1,"LVM",1,"1LE10030EA022JA5"]
["1LE1003-0EA40-4GB5","SIMOTICS GP MOTOR TYPE: 1AV3094A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 90L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF165 (A200) MOTOR PROTECTION WITH 1 PTC THERMISTORS FOR SHUTDOWN Terminal box lateral right",512,"ΤΕΜ",1,"LVM",1,"1LE10030EA404GB5"]
["1LE1003-0EA43-4AA5","SIMOTICS GP MOTOR TYPE: 1AV3094A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 90L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, WITHOUT MOTOR PROTECTION Terminal box lateral right",467,"ΤΕΜ",1,"LVM",1,"1LE10030EA434AA5"]
["1LE1003-0EB00-4GA6","SIMOTICS GP MOTOR TYPE: 1AV3090B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 90S * 1.1kW (50 Hz) 1.27kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF165 (A200) WITHOUT MOTOR PROTECTION Terminal box lateral left",385,"ΤΕΜ",1,"LVM",1,"1LE10030EB004GA6"]
["1LE1003-0EB03-3FA5","SIMOTICS GP MOTOR TYPE: 1AV3090B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 90S * 1.1kW (50 Hz) 1.27kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 5, flange: FF165 (A200) WITHOUT MOTOR PROTECTION Terminal box lateral right",403,"ΤΕΜ",1,"LVM",1,"1LE10030EB033FA5"]
["1LE1003-0EB43-3GB5","SIMOTICS GP MOTOR TYPE: 1AV3094B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 90L * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF165 (A200) MOTOR PROTECTION WITH 1 PTC THERMISTORS FOR SHUTDOWN Terminal box lateral right",483,"ΤΕΜ",1,"LVM",1,"1LE10030EB433GB5"]
["1LE1003-0EC00-4JA5","SIMOTICS GP MOTOR TYPE: 1AV3090C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 6-pole * Size 90S * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF165 (A200) without motor protection Terminal box lateral right",378,"ΤΕΜ",1,"LVM",1,"1LE10030EC004JA5"]
["1LE1003-0EC02-2AA5","SIMOTICS GP MOTOR TYPE: 1AV3090C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 6-pole * Size 90S * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, without motor protection Terminal box lateral right",350,"ΤΕΜ",1,"LVM",1,"1LE10030EC022AA5"]
["1LE1003-0EC40-4GB5","SIMOTICS GP MOTOR TYPE: 1AV3094C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE1 6-pole * Size 90L * 1.1kW (50 Hz) 1.27kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF165 (A200) 1 PTC thermistor for disconnection (2 terminals) Terminal box lateral right",475,"ΤΕΜ",1,"LVM",1,"1LE10030EC404GB5"]
["1LE1003-0EC43-4FA4","SIMOTICS GP MOTOR TYPE: 1AV3094C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE1 6-pole * Size 90L * 1.1kW (50 Hz) 1.27kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF165 (A200) without motor protection Terminal box at top",440,"ΤΕΜ",1,"LVM",1,"1LE10030EC434FA4"]
["1LE1003-1AA42-1FA7","SIMOTICS GP MOTOR TYPE: 1AV3104A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF215 (A250) Without motor protection Terminal box below",597,"ΤΕΜ",1,"LVM",1,"1LE10031AA421FA7"]
["1LE1003-1AA43-4GB5","SIMOTICS GP MOTOR TYPE: 1AV3104A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",624,"ΤΕΜ",1,"LVM",1,"1LE10031AA434GB5"]
["1LE1003-1AB42-2AA5","SIMOTICS GP MOTOR TYPE: 1AV3104B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 100L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 Without motor protection Terminal box on RHS",498,"ΤΕΜ",1,"LVM",1,"1LE10031AB422AA5"]
["1LE1003-1AB43-3FA6","SIMOTICS GP MOTOR TYPE: 1AV3104B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 100L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 5, flange: FF215 (A250) Without motor protection Terminal box on left-hand side",555,"ΤΕΜ",1,"LVM",1,"1LE10031AB433FA6"]
["1LE1003-1AB43-4FC4","SIMOTICS GP MOTOR TYPE: 1AV3104B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 100L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF215 (A250) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",574,"ΤΕΜ",1,"LVM",1,"1LE10031AB434FC4"]
["1LE1003-1AB52-2AC5","SIMOTICS GP MOTOR TYPE: 1AV3105B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",655,"ΤΕΜ",1,"LVM",1,"1LE10031AB522AC5"]
["1LE1003-1AB53-4AB7","SIMOTICS GP MOTOR TYPE: 1AV3105B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box below",619,"ΤΕΜ",1,"LVM",1,"1LE10031AB534AB7"]
["1LE1003-1AC42-1JB7","SIMOTICS GP MOTOR TYPE: 1AV3104C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 100L * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",604,"ΤΕΜ",1,"LVM",1,"1LE10031AC421JB7"]
["1LE1003-1AC43-4JA7","SIMOTICS GP MOTOR TYPE: 1AV3104C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 100L * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF215 (A250) without motor protection Terminal box below",531,"ΤΕΜ",1,"LVM",1,"1LE10031AC434JA7"]
["1LE1003-1BA22-1GA7","SIMOTICS GP MOTOR TYPE: 1AV3112A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF215 (A250) Without motor protection Terminal box below",706,"ΤΕΜ",1,"LVM",1,"1LE10031BA221GA7"]
["1LE1003-1BA23-3JA4","SIMOTICS GP MOTOR TYPE: 1AV3112A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 35, flange: FF215 (A250) Without motor protection Terminal box at top",662,"ΤΕΜ",1,"LVM",1,"1LE10031BA233JA4"]
["1LE1003-1BB22-1AB7","SIMOTICS GP MOTOR TYPE: 1AV3112B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box below",764,"ΤΕΜ",1,"LVM",1,"1LE10031BB221AB7"]
["1LE1003-1BB22-2GA4","SIMOTICS GP MOTOR TYPE: 1AV3112B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF215 (A250) Without motor protection Terminal box at top",681,"ΤΕΜ",1,"LVM",1,"1LE10031BB222GA4"]
["1LE1003-1BC20-4JB4","SIMOTICS GP MOTOR TYPE: 1AV3112C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 112M, * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",668,"ΤΕΜ",1,"LVM",1,"1LE10031BC204JB4"]
["1LE1003-1BC22-1GA5","SIMOTICS GP MOTOR TYPE: 1AV3112C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 112M, * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF215 (A250) without motor protection Terminal box on RHS",689,"ΤΕΜ",1,"LVM",1,"1LE10031BC221GA5"]
["1LE1003-1CA00-4AB5","SIMOTICS GP MOTOR TYPE: 1AV3130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",863,"ΤΕΜ",1,"LVM",1,"1LE10031CA004AB5"]
["1LE1003-1CA02-1AA6","SIMOTICS GP MOTOR TYPE: 1AV3130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B3 Without motor protection Terminal box on left-hand side",822,"ΤΕΜ",1,"LVM",1,"1LE10031CA021AA6"]
["1LE1003-1CA03-3GA6","SIMOTICS GP MOTOR TYPE: 1AV3130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF265 (A300) Without motor protection Terminal box on left-hand side",878,"ΤΕΜ",1,"LVM",1,"1LE10031CA033GA6"]
["1LE1003-1CA03-4WC7","SIMOTICS GP MOTOR TYPE: 1AV3130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF265 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",972,"ΤΕΜ",1,"LVM",1,"1LE10031CA034WC7"]
["1LE1003-1CA12-2JB6","SIMOTICS GP MOTOR TYPE: 1AV3131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1122,"ΤΕΜ",1,"LVM",1,"1LE10031CA122JB6"]
["1LE1003-1CA13-3GB6","SIMOTICS GP MOTOR TYPE: 1AV3131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1155,"ΤΕΜ",1,"LVM",1,"1LE10031CA133GB6"]
["1LE1003-1CB02-1WB5","SIMOTICS GP MOTOR TYPE: 1AV3130B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 15 * Flange: FF265 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",1035,"ΤΕΜ",1,"LVM",1,"1LE10031CB021WB5"]
["1LE1003-1CB03-3JA7","SIMOTICS GP MOTOR TYPE: 1AV3130B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 35, flange: FF265 (A300) Without motor protection Terminal box below",947,"ΤΕΜ",1,"LVM",1,"1LE10031CB033JA7"]
["1LE1003-1CB03-4JA6","SIMOTICS GP MOTOR TYPE: 1AV3130B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35, flange: FF265 (A300) Without motor protection Terminal box on left-hand side",912,"ΤΕΜ",1,"LVM",1,"1LE10031CB034JA6"]
["1LE1003-1CB22-2AB7","SIMOTICS GP MOTOR TYPE: 1AV3132B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 132M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1144,"ΤΕΜ",1,"LVM",1,"1LE10031CB222AB7"]
["1LE1003-1CB23-3JB7","SIMOTICS GP MOTOR TYPE: 1AV3132B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 132M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 35, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1237,"ΤΕΜ",1,"LVM",1,"1LE10031CB233JB7"]
["1LE1003-1CC00-4FB5","SIMOTICS GP MOTOR TYPE: 1AV3130C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 132S, * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",893,"ΤΕΜ",1,"LVM",1,"1LE10031CC004FB5"]
["1LE1003-1CC02-3JB6","SIMOTICS GP MOTOR TYPE: 1AV3130C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 132S, * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 240 VD/415 VY 3 AC 60 Hz 480 VY IM B 35 * Flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",930,"ΤΕΜ",1,"LVM",1,"1LE10031CC023JB6"]
["1LE1003-1CC03-4GA6","SIMOTICS GP MOTOR TYPE: 1AV3130C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 132S, * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF265 (A300) without motor protection Terminal box on left-hand side",817,"ΤΕΜ",1,"LVM",1,"1LE10031CC034GA6"]
["1LE1003-1CC22-1AB7","SIMOTICS GP MOTOR TYPE: 1AV3132C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 132M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1041,"ΤΕΜ",1,"LVM",1,"1LE10031CC221AB7"]
["1LE1503-1DA22-1GA6","SIMOTICS SD MOTOR TYPE: 1CV3162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF300 (A350) without motor protection Terminal box on left-hand side",1582,"ΤΕΜ",1,"LVM",1,"1LE15031DA221GA6"]
["1LE1503-1DA23-3JB4","SIMOTICS SD MOTOR TYPE: 1CV3162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1610,"ΤΕΜ",1,"LVM",1,"1LE15031DA233JB4"]
["1LE1503-1DA23-4JC4","SIMOTICS SD MOTOR TYPE: 1CV3162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",1606,"ΤΕΜ",1,"LVM",1,"1LE15031DA234JC4"]
["1LE1503-1DA32-2JC7","SIMOTICS SD MOTOR TYPE: 1CV3163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",2098,"ΤΕΜ",1,"LVM",1,"1LE15031DA322JC7"]
["1LE1503-1DA42-2GC5","SIMOTICS SD MOTOR TYPE: 1CV3164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",2439,"ΤΕΜ",1,"LVM",1,"1LE15031DA422GC5"]
["1LE1503-1DA43-4AA6","SIMOTICS SD MOTOR TYPE: 1CV3164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box on left-hand side",2253,"ΤΕΜ",1,"LVM",1,"1LE15031DA434AA6"]
["1LE1503-1EA22-2AB6","SIMOTICS SD MOTOR TYPE: 1CV3182A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 180M, * 22kW (50 Hz) 24.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",2639,"ΤΕΜ",1,"LVM",1,"1LE15031EA222AB6"]
["1LE1503-1EA23-4GB5","SIMOTICS SD MOTOR TYPE: 1CV3182A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 180M, * 22kW (50 Hz) 24.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",2751,"ΤΕΜ",1,"LVM",1,"1LE15031EA234GB5"]
["1LE1503-1EB22-2JA4","SIMOTICS SD MOTOR TYPE: 1CV3182B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 4-pole * Size 180M, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2178,"ΤΕΜ",1,"LVM",1,"1LE15031EB222JA4"]
["1LE1503-1EB23-3GA5","SIMOTICS SD MOTOR TYPE: 1CV3182B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 4-pole * Size 180M, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF300 (A350) without motor protection Terminal box on RHS",2373,"ΤΕΜ",1,"LVM",1,"1LE15031EB233GA5"]
["1LE1503-1EB42-2WC5","SIMOTICS SD MOTOR TYPE: 1CV3184B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 4-pole * Size 180L, * 22kW (50 Hz) 25.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 15 * Flange: FF300 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",2863,"ΤΕΜ",1,"LVM",1,"1LE15031EB422WC5"]
["1LE1503-1EC40-4FB6","SIMOTICS SD MOTOR TYPE: 1CV3184C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 180L, * 15kW (50 Hz) 18kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",2906,"ΤΕΜ",1,"LVM",1,"1LE15031EC404FB6"]
["1LE1503-1EC43-3FB5","SIMOTICS SD MOTOR TYPE: 1CV3184C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 180L, * 15kW (50 Hz) 18kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",2965,"ΤΕΜ",1,"LVM",1,"1LE15031EC433FB5"]
["1LE1503-1EC43-4AC4","SIMOTICS SD MOTOR TYPE: 1CV3184C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 180L, * 15kW (50 Hz) 18kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",2714,"ΤΕΜ",1,"LVM",1,"1LE15031EC434AC4"]
["1LE1503-2AA42-2AB5","SIMOTICS SD MOTOR TYPE: 1CV3204A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 200L, * 30kW (50 Hz) 33.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",3409,"ΤΕΜ",1,"LVM",1,"1LE15032AA422AB5"]
["1LE1503-2AA43-4GA6","SIMOTICS SD MOTOR TYPE: 1CV3204A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 200L, * 30kW (50 Hz) 33.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF350 (A400) without motor protection Terminal box on left-hand side",3445,"ΤΕΜ",1,"LVM",1,"1LE15032AA434GA6"]
["1LE1503-2AA52-1FA4","SIMOTICS SD MOTOR TYPE: 1CV3205A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 200L, * 37kW (50 Hz) 41.5kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF350 (A400) without motor protection Terminal box at top",4127,"ΤΕΜ",1,"LVM",1,"1LE15032AA521FA4"]
["1LE1503-2AA53-4JB5","SIMOTICS SD MOTOR TYPE: 1CV3205A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 200L, * 37kW (50 Hz) 41.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",4384,"ΤΕΜ",1,"LVM",1,"1LE15032AA534JB5"]
["1LE1503-2AB52-2JC6","SIMOTICS SD MOTOR TYPE: 1CV3205B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 200L, * 30kW (50 Hz) 34.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF350 (A400) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",3620,"ΤΕΜ",1,"LVM",1,"1LE15032AB522JC6"]
["1LE1503-2AB53-3GB5","SIMOTICS SD MOTOR TYPE: 1CV3205B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 200L, * 30kW (50 Hz) 34.5kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",3570,"ΤΕΜ",1,"LVM",1,"1LE15032AB533GB5"]
["1LE1503-2AC43-3FA5","SIMOTICS SD MOTOR TYPE: 1CV3204C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 200L, * 18.5 kW (50 Hz) 22 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 5, flange: FF350 (A400) without motor protection Terminal box on RHS",3487,"ΤΕΜ",1,"LVM",1,"1LE15032AC433FA5"]
["1LE1503-2AC43-4FC6","SIMOTICS SD MOTOR TYPE: 1CV3204C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 200L, * 18.5 kW (50 Hz) 22 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF350 (A400) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",3597,"ΤΕΜ",1,"LVM",1,"1LE15032AC434FC6"]
["1LE1503-2AC52-1FA6","SIMOTICS SD MOTOR TYPE: 1CV3205C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 200L, * 22kW (50 Hz) 26.5kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF350 (A400) without motor protection Terminal box on left-hand side",3975,"ΤΕΜ",1,"LVM",1,"1LE15032AC521FA6"]
["1LE1503-2BA22-1FA6","SIMOTICS SD MOTOR TYPE: 1CV3222A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 225M * 45kW (50 Hz) 51kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF400 (A450) without motor protection Terminal box on left-hand side",4895,"ΤΕΜ",1,"LVM",1,"1LE15032BA221FA6"]
["1LE1503-2BA22-2GC6","SIMOTICS SD MOTOR TYPE: 1CV3222A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 225M * 45kW (50 Hz) 51kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF400 (A450) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",5036,"ΤΕΜ",1,"LVM",1,"1LE15032BA222GC6"]
["1LE1503-2BB00-4FB4","SIMOTICS SD MOTOR TYPE: 1CV3220B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 225S * 37kW (50 Hz) 42.5kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF400 (A450) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",3842,"ΤΕΜ",1,"LVM",1,"1LE15032BB004FB4"]
["1LE1503-2BB02-2WB4","SIMOTICS SD MOTOR TYPE: 1CV3220B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 225S * 37kW (50 Hz) 42.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 15 * Flange: FF400 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",3962,"ΤΕΜ",1,"LVM",1,"1LE15032BB022WB4"]
["1LE1503-2BB22-1AA6","SIMOTICS SD MOTOR TYPE: 1CV3222B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 225M * 45kW (50 Hz) 52kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, without motor protection Terminal box on left-hand side",4462,"ΤΕΜ",1,"LVM",1,"1LE15032BB221AA6"]
["1LE1503-2BB22-1WB6","SIMOTICS SD MOTOR TYPE: 1CV3222B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 225M * 45kW (50 Hz) 52kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 15 * Flange: FF400 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",4895,"ΤΕΜ",1,"LVM",1,"1LE15032BB221WB6"]
["1LE1503-2BB23-3WB5","SIMOTICS SD MOTOR TYPE: 1CV3222B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 225M * 45kW (50 Hz) 52kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 15 * Flange: FF400 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",4895,"ΤΕΜ",1,"LVM",1,"1LE15032BB233WB5"]
["1LE1503-2BC23-3GA5","SIMOTICS SD MOTOR TYPE: 1CV3222C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 225M * 30kW (50 Hz) 36 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF400 (A450) without motor protection Terminal box on RHS",5022,"ΤΕΜ",1,"LVM",1,"1LE15032BC233GA5"]
["1LE1503-2BC23-4FA5","SIMOTICS SD MOTOR TYPE: 1CV3222C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 225M * 30kW (50 Hz) 36 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF400 (A450) without motor protection Terminal box on RHS",4931,"ΤΕΜ",1,"LVM",1,"1LE15032BC234FA5"]
["1LE1503-2CA22-2FC5","SIMOTICS SD MOTOR TYPE: 1CV3252A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 250M * 55kW (50 Hz) 62kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF500 (A550) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",6058,"ΤΕΜ",1,"LVM",1,"1LE15032CA222FC5"]
["1LE1503-2CA23-4JB6","SIMOTICS SD MOTOR TYPE: 1CV3252A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 250M * 55kW (50 Hz) 62kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",6060,"ΤΕΜ",1,"LVM",1,"1LE15032CA234JB6"]
["1LE1503-2CB22-2GC6","SIMOTICS SD MOTOR TYPE: 1CV3252B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 250M * 55kW (50 Hz) 63kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF500 (A550) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",5768,"ΤΕΜ",1,"LVM",1,"1LE15032CB222GC6"]
["1LE1503-2CB23-4FA5","SIMOTICS SD MOTOR TYPE: 1CV3252B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 250M * 55kW (50 Hz) 63kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF500 (A550) without motor protection Terminal box on RHS",5534,"ΤΕΜ",1,"LVM",1,"1LE15032CB234FA5"]
["1LE1503-2CC22-2JC6","SIMOTICS SD MOTOR TYPE: 1CV3252C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 250M * 37kW (50 Hz) 44.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF500 (A550) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",6448,"ΤΕΜ",1,"LVM",1,"1LE15032CC222JC6"]
["1LE1503-2DA00-4JB6","SIMOTICS SD MOTOR TYPE: 1CV3280A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 280S, * 75kW (50 Hz) 84kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",8029,"ΤΕΜ",1,"LVM",1,"1LE15032DA004JB6"]
["1LE1503-2DA03-3AB4","SIMOTICS SD MOTOR TYPE: 1CV3280A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 280S, * 75kW (50 Hz) 84kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",7402,"ΤΕΜ",1,"LVM",1,"1LE15032DA033AB4"]
["1LE1503-2DA03-3WB4","SIMOTICS SD MOTOR TYPE: 1CV3280A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 280S, * 75kW (50 Hz) 84kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 15 * Flange: FF500 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",7927,"ΤΕΜ",1,"LVM",1,"1LE15032DA033WB4"]
["1LE1503-2DA22-2GA5","SIMOTICS SD MOTOR TYPE: 1CV3282A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 280M * 90kW (50 Hz) 101kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF500 (A550) without motor protection Terminal box on RHS",9075,"ΤΕΜ",1,"LVM",1,"1LE15032DA222GA5"]
["1LE1503-2DA23-4GC4","SIMOTICS SD MOTOR TYPE: 1CV3282A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 280M * 90kW (50 Hz) 101kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF500 (A550) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",8997,"ΤΕΜ",1,"LVM",1,"1LE15032DA234GC4"]
["1LE1503-2DB02-2FC6","SIMOTICS SD MOTOR TYPE: 1CV3280B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 280S, * 75kW (50 Hz) 86kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF500 (A550) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",7678,"ΤΕΜ",1,"LVM",1,"1LE15032DB022FC6"]
["1LE1503-2DB20-4GA5","SIMOTICS SD MOTOR TYPE: 1CV3282B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 280M * 90kW (50 Hz) 104kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF500 (A550) without motor protection Terminal box on RHS",8571,"ΤΕΜ",1,"LVM",1,"1LE15032DB204GA5"]
["1LE1503-2DB23-4FA4","SIMOTICS SD MOTOR TYPE: 1CV3282B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 280M * 90kW (50 Hz) 104kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF500 (A550) without motor protection Terminal box at top",8206,"ΤΕΜ",1,"LVM",1,"1LE15032DB234FA4"]
["1LE1503-2DC02-2AC5","SIMOTICS SD MOTOR TYPE: 1CV3280C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 280S, * 45kW (50 Hz) 54kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",7368,"ΤΕΜ",1,"LVM",1,"1LE15032DC022AC5"]
["1LE1503-2DC03-4GC5","SIMOTICS SD MOTOR TYPE: 1CV3280C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 280S, * 45kW (50 Hz) 54kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF500 (A550) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",7680,"ΤΕΜ",1,"LVM",1,"1LE15032DC034GC5"]
["1LE1503-2DC22-1FA6","SIMOTICS SD MOTOR TYPE: 1CV3282C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 280M * 55kW (50 Hz) 66kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF500 (A550) without motor protection Terminal box on left-hand side",8702,"ΤΕΜ",1,"LVM",1,"1LE15032DC221FA6"]
["1LE1503-2DC23-3FB6","SIMOTICS SD MOTOR TYPE: 1CV3282C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 280M * 55kW (50 Hz) 66kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 5, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",8873,"ΤΕΜ",1,"LVM",1,"1LE15032DC233FB6"]
["1LE1503-3AA03-3FA5","SIMOTICS SD MOTOR TYPE: 1CV3310A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 315S, * 110kW (50 Hz) 123kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 5, Flange: FF600 (A660) without motor protection Terminal box on RHS",11112,"ΤΕΜ",1,"LVM",1,"1LE15033AA033FA5"]
["1LE1503-3AA03-4FA4","SIMOTICS SD MOTOR TYPE: 1CV3310A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 315S, * 110kW (50 Hz) 123kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, Flange: FF600 (A660) without motor protection Terminal box at top",10521,"ΤΕΜ",1,"LVM",1,"1LE15033AA034FA4"]
["1LE1503-3AA22-2AA5","SIMOTICS SD MOTOR TYPE: 1CV3312A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 315M, * 132kW (50 Hz) 148kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, without motor protection Terminal box on RHS",12514,"ΤΕΜ",1,"LVM",1,"1LE15033AA222AA5"]
["1LE1503-3AA42-1GA5","SIMOTICS SD MOTOR TYPE: 1CV3314A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 315L, * 160kW (50 Hz) 180kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, Flange: FF600 (A660) without motor protection Terminal box on RHS",16215,"ΤΕΜ",1,"LVM",1,"1LE15033AA421GA5"]
["1LE1503-3AA50-4GB6","SIMOTICS SD MOTOR TYPE: 1CV3315A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 315L, * 200kW (50 Hz) 224kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",19950,"ΤΕΜ",1,"LVM",1,"1LE15033AA504GB6"]
["1LE1503-3AA52-2JA4","SIMOTICS SD MOTOR TYPE: 1CV3315A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 315L, * 200kW (50 Hz) 224kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF600 (A660) without motor protection Terminal box at top",19236,"ΤΕΜ",1,"LVM",1,"1LE15033AA522JA4"]
["1LE1503-3AB02-2JC5","SIMOTICS SD MOTOR TYPE: 1CV3310B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 4-pole * Size 315S, * 110kW (50 Hz) 127kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF600 (A660) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",11077,"ΤΕΜ",1,"LVM",1,"1LE15033AB022JC5"]
["1LE1503-3AB20-4FB5","SIMOTICS SD MOTOR TYPE: 1CV3312B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 4-pole * Size 315M, * 132kW (50 Hz) 152kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",12663,"ΤΕΜ",1,"LVM",1,"1LE15033AB204FB5"]
["1LE1503-3AB23-3GB4","SIMOTICS SD MOTOR TYPE: 1CV3312B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 4-pole * Size 315M, * 132kW (50 Hz) 152kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",12423,"ΤΕΜ",1,"LVM",1,"1LE15033AB233GB4"]
["1LE1503-3AB23-4JA5","SIMOTICS SD MOTOR TYPE: 1CV3312B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 4-pole * Size 315M, * 132kW (50 Hz) 152kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF600 (A660) without motor protection Terminal box on RHS",12556,"ΤΕΜ",1,"LVM",1,"1LE15033AB234JA5"]
["1LE1503-3AB43-4GC4","SIMOTICS SD MOTOR TYPE: 1CV3314B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 4-pole * Size 315L, * 160kW (50 Hz) 184kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, Flange: FF600 (A660) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",14843,"ΤΕΜ",1,"LVM",1,"1LE15033AB434GC4"]
["1LE1503-3AB52-2JB6","SIMOTICS SD MOTOR TYPE: 1CV3315B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 315L, * 200kW (50 Hz) 230kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",18606,"ΤΕΜ",1,"LVM",1,"1LE15033AB522JB6"]
["1LE1503-3AC00-4JB6","SIMOTICS SD MOTOR TYPE: 1CV3310C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 6-pole * Size 315S, * 75kW (50 Hz) 90 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",11802,"ΤΕΜ",1,"LVM",1,"1LE15033AC004JB6"]
["1LE1503-3AC23-4FA4","SIMOTICS SD MOTOR TYPE: 1CV3312C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 315M, * 90kW (50 Hz) 108kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, Flange: FF600 (A660) without motor protection Terminal box at top",12537,"ΤΕΜ",1,"LVM",1,"1LE15033AC234FA4"]
["1LE1503-3AC52-2JC4","SIMOTICS SD MOTOR TYPE: 1CV3315C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 315L, * 132kW (50 Hz) 158kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF600 (A660) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",18094,"ΤΕΜ",1,"LVM",1,"1LE15033AC522JC4"]
["1LE1503-3AC63-4JC5","SIMOTICS SD MOTOR TYPE: 1CV3316C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 315L, * 160kW (50 Hz) 192kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF600 (A660) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",22207,"ΤΕΜ",1,"LVM",1,"1LE15033AC634JC5"]
["1LE1504-1CA13-4JB6","SIMOTICS SD MOTOR TYPE: 1CV4131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1424,"ΤΕΜ",1,"LVM",1,"1LE15041CA134JB6"]
["1LE1504-1DA42-2GC7","SIMOTICS SD MOTOR TYPE: 1CV4164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",2901,"ΤΕΜ",1,"LVM",1,"1LE15041DA422GC7"]
["1LE1504-1EA22-2FC4","SIMOTICS SD MOTOR TYPE: 1CV4182A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 180M, * 22kW (50 Hz) 24.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",3213,"ΤΕΜ",1,"LVM",1,"1LE15041EA222FC4"]
["1LE1504-1EA22-2JA4","SIMOTICS SD MOTOR TYPE: 1CV4182A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 180M, * 22kW (50 Hz) 24.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",3056,"ΤΕΜ",1,"LVM",1,"1LE15041EA222JA4"]
["1LE1504-1EB22-1AA5","SIMOTICS SD MOTOR TYPE: 1CV4182B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 180M, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, without motor protection Terminal box on RHS",2693,"ΤΕΜ",1,"LVM",1,"1LE15041EB221AA5"]
["1LE1504-1EB23-3AB4","SIMOTICS SD MOTOR TYPE: 1CV4182B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 180M, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2637,"ΤΕΜ",1,"LVM",1,"1LE15041EB233AB4"]
["1LE1504-1EB42-1GA6","SIMOTICS SD MOTOR TYPE: 1CV4184B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 180L, * 22kW (50 Hz) 25.3kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF300 (A350) without motor protection Terminal box on left-hand side",3183,"ΤΕΜ",1,"LVM",1,"1LE15041EB421GA6"]
["1LE1504-1EB43-3FB6","SIMOTICS SD MOTOR TYPE: 1CV4184B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 180L, * 22kW (50 Hz) 25.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",3284,"ΤΕΜ",1,"LVM",1,"1LE15041EB433FB6"]
["1LE1504-2AA40-4GA5","SIMOTICS SD MOTOR TYPE: 1CV4204A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 200L, * 30kW (50 Hz) 33.5kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF350 (A400) without motor protection Terminal box on RHS",4041,"ΤΕΜ",1,"LVM",1,"1LE15042AA404GA5"]
["1LE1504-2AA43-4GC4","SIMOTICS SD MOTOR TYPE: 1CV4204A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 200L, * 30kW (50 Hz) 33.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF350 (A400) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",4035,"ΤΕΜ",1,"LVM",1,"1LE15042AA434GC4"]
["1LE1504-2AA52-1WB5","SIMOTICS SD MOTOR TYPE: 1CV4205A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 200L, * 37kW (50 Hz) 41.5kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 15 * Flange: FF350 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",5214,"ΤΕΜ",1,"LVM",1,"1LE15042AA521WB5"]
["1LE1504-2AA53-4FB6","SIMOTICS SD MOTOR TYPE: 1CV4205A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 200L, * 37kW (50 Hz) 41.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",5083,"ΤΕΜ",1,"LVM",1,"1LE15042AA534FB6"]
["1LE1504-2AB52-2AC4","SIMOTICS SD MOTOR TYPE: 1CV4205B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 200L, * 30kW (50 Hz) 34.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",3857,"ΤΕΜ",1,"LVM",1,"1LE15042AB522AC4"]
["1LE1504-2AB53-3GA5","SIMOTICS SD MOTOR TYPE: 1CV4205B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 200L, * 30kW (50 Hz) 34.5kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF350 (A400) without motor protection Terminal box on RHS",4066,"ΤΕΜ",1,"LVM",1,"1LE15042AB533GA5"]
["1LE1504-2BA20-4JA4","SIMOTICS SD MOTOR TYPE: 1CV4222A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 225M * 45kW (50 Hz) 51kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF400 (A450) without motor protection Terminal box at top",5303,"ΤΕΜ",1,"LVM",1,"1LE15042BA204JA4"]
["1LE1504-2BA22-2GC6","SIMOTICS SD MOTOR TYPE: 1CV4222A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 225M * 45kW (50 Hz) 51kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF400 (A450) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",5708,"ΤΕΜ",1,"LVM",1,"1LE15042BA222GC6"]
["1LE1504-2BB00-4WB6","SIMOTICS SD MOTOR TYPE: 1CV4220B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 225S * 37kW (50 Hz) 42.5kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF400 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",4758,"ΤΕΜ",1,"LVM",1,"1LE15042BB004WB6"]
["1LE1504-2BB03-4AB6","SIMOTICS SD MOTOR TYPE: 1CV4220B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 225S * 37kW (50 Hz) 42.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",4462,"ΤΕΜ",1,"LVM",1,"1LE15042BB034AB6"]
["1LE1504-2BB22-1GA4","SIMOTICS SD MOTOR TYPE: 1CV4222B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 60 Hz, P60: IE3 4-pole * Size 225M * 45kW (50 Hz) 52kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF400 (A450) without motor protection Terminal box at top",5057,"ΤΕΜ",1,"LVM",1,"1LE15042BB221GA4"]
["1LE1504-2BB23-4FB5","SIMOTICS SD MOTOR TYPE: 1CV4222B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 60 Hz, P60: IE3 4-pole * Size 225M * 45kW (50 Hz) 52kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF400 (A450) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",5319,"ΤΕΜ",1,"LVM",1,"1LE15042BB234FB5"]
["1LE1504-2CA20-4FB6","SIMOTICS SD MOTOR TYPE: 1CV4252A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 250M * 55kW (50 Hz) 62kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",6720,"ΤΕΜ",1,"LVM",1,"1LE15042CA204FB6"]
["1LE1504-2CA22-2FA4","SIMOTICS SD MOTOR TYPE: 1CV4252A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 250M * 55kW (50 Hz) 62kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF500 (A550) without motor protection Terminal box at top",6261,"ΤΕΜ",1,"LVM",1,"1LE15042CA222FA4"]
["1LE1504-2CB20-4AA4","SIMOTICS SD MOTOR TYPE: 1CV4252B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 250M * 55kW (50 Hz) 63kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B3 without motor protection Terminal box at top",5796,"ΤΕΜ",1,"LVM",1,"1LE15042CB204AA4"]
["1LE1504-2CB22-2AA4","SIMOTICS SD MOTOR TYPE: 1CV4252B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 250M * 55kW (50 Hz) 63kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 without motor protection Terminal box at top",5796,"ΤΕΜ",1,"LVM",1,"1LE15042CB222AA4"]
["1LE1504-2DA00-4FB4","SIMOTICS SD MOTOR TYPE: 1CV4280A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 280S, * 75kW (50 Hz) 84kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",8713,"ΤΕΜ",1,"LVM",1,"1LE15042DA004FB4"]
["1LE1504-2DA03-3GB5","SIMOTICS SD MOTOR TYPE: 1CV4280A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 280S, * 75kW (50 Hz) 84kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",9210,"ΤΕΜ",1,"LVM",1,"1LE15042DA033GB5"]
["1LE1504-2DA20-4GB6","SIMOTICS SD MOTOR TYPE: 1CV4282A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 280M * 90kW (50 Hz) 101kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",10505,"ΤΕΜ",1,"LVM",1,"1LE15042DA204GB6"]
["1LE1504-2DA23-3AA4","SIMOTICS SD MOTOR TYPE: 1CV4282A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 280M * 90kW (50 Hz) 101kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, without motor protection Terminal box at top",9794,"ΤΕΜ",1,"LVM",1,"1LE15042DA233AA4"]
["1LE1504-2DB02-1WB5","SIMOTICS SD MOTOR TYPE: 1CV4280B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 280S, * 75kW (50 Hz) 86kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 15 * Flange: FF500 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",8962,"ΤΕΜ",1,"LVM",1,"1LE15042DB021WB5"]
["1LE1504-2DB02-2GB5","SIMOTICS SD MOTOR TYPE: 1CV4280B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 280S, * 75kW (50 Hz) 86kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",8615,"ΤΕΜ",1,"LVM",1,"1LE15042DB022GB5"]
["1LE1504-2DB22-2JB5","SIMOTICS SD MOTOR TYPE: 1CV4282B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 280M * 90kW (50 Hz) 104kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",9919,"ΤΕΜ",1,"LVM",1,"1LE15042DB222JB5"]
["1LE1504-2DB23-3FA4","SIMOTICS SD MOTOR TYPE: 1CV4282B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 280M * 90kW (50 Hz) 104kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 5, flange: FF500 (A550) without motor protection Terminal box at top",9432,"ΤΕΜ",1,"LVM",1,"1LE15042DB233FA4"]
["1LE1504-3AA02-2GC4","SIMOTICS SD MOTOR TYPE: 1CV4310A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 315S, * 110kW (50 Hz) 123kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, Flange: FF600 (A660) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",12155,"ΤΕΜ",1,"LVM",1,"1LE15043AA022GC4"]
["1LE1504-3AA03-4FA6","SIMOTICS SD MOTOR TYPE: 1CV4310A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 315S, * 110kW (50 Hz) 123kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, Flange: FF600 (A660) without motor protection Terminal box on left-hand side",12283,"ΤΕΜ",1,"LVM",1,"1LE15043AA034FA6"]
["1LE1504-3AA23-3AA6","SIMOTICS SD MOTOR TYPE: 1CV4312A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 315M, * 132kW (50 Hz) 148kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, without motor protection Terminal box on left-hand side",14241,"ΤΕΜ",1,"LVM",1,"1LE15043AA233AA6"]
["1LE1504-3AA40-4GA4","SIMOTICS SD MOTOR TYPE: 1CV4314A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 315L, * 160kW (50 Hz) 180kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, Flange: FF600 (A660) without motor protection Terminal box at top",17682,"ΤΕΜ",1,"LVM",1,"1LE15043AA404GA4"]
["1LE1504-3AA50-4JA5","SIMOTICS SD MOTOR TYPE: 1CV4315A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 315L, * 200kW (50 Hz) 224kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF600 (A660) without motor protection Terminal box on RHS",22174,"ΤΕΜ",1,"LVM",1,"1LE15043AA504JA5"]
["1LE1504-3AB00-4FB4","SIMOTICS SD MOTOR TYPE: 1CV4310B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 315M, * 110kW (50 Hz) 127kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",11784,"ΤΕΜ",1,"LVM",1,"1LE15043AB004FB4"]
["1LE1504-3AB02-1AB6","SIMOTICS SD MOTOR TYPE: 1CV4310B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 315M, * 110kW (50 Hz) 127kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",11933,"ΤΕΜ",1,"LVM",1,"1LE15043AB021AB6"]
["1LE1504-3AB20-4AA6","SIMOTICS SD MOTOR TYPE: 1CV4312B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 315M, * 132kW (50 Hz) 152kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box on left-hand side",13522,"ΤΕΜ",1,"LVM",1,"1LE15043AB204AA6"]
["1LE1504-3AB22-2FA5","SIMOTICS SD MOTOR TYPE: 1CV4312B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 315M, * 132kW (50 Hz) 152kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, Flange: FF600 (A660) without motor protection Terminal box on RHS",13963,"ΤΕΜ",1,"LVM",1,"1LE15043AB222FA5"]
["1LE1504-3AB23-4GA6","SIMOTICS SD MOTOR TYPE: 1CV4312B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 315M, * 132kW (50 Hz) 152kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, Flange: FF600 (A660) without motor protection Terminal box on left-hand side",13967,"ΤΕΜ",1,"LVM",1,"1LE15043AB234GA6"]
["1LE1504-3AB43-3AA6","SIMOTICS SD MOTOR TYPE: 1CV4314B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 315L, * 160kW (50 Hz) 184kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, without motor protection Terminal box on left-hand side",16467,"ΤΕΜ",1,"LVM",1,"1LE15043AB433AA6"]
["1LE1504-3AB53-4AA4","SIMOTICS SD MOTOR TYPE: 1CV4315B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 315L, * 200kW (50 Hz) 230kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box at top",19740,"ΤΕΜ",1,"LVM",1,"1LE15043AB534AA4"]
["1LE1601-1EA22-1GB5","SIMOTICS SD MOTOR TYPE: 1CV2182A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 180M, * 22kW (50 Hz) 24.5kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",2730,"ΤΕΜ",1,"LVM",1,"1LE16011EA221GB5"]
["1LE1601-1EB22-2GC5","SIMOTICS SD MOTOR TYPE: 1CV2182B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 180M, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",2483,"ΤΕΜ",1,"LVM",1,"1LE16011EB222GC5"]
["1LE1601-1EB42-2GB4","SIMOTICS SD MOTOR TYPE: 1CV2184B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 180L, * 22kW (50 Hz) 25.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2478,"ΤΕΜ",1,"LVM",1,"1LE16011EB422GB4"]
["1LE1601-2AA42-1GB4","SIMOTICS SD MOTOR TYPE: 1CV2204A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 200L, * 30kW (50 Hz) 33.5kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",3316,"ΤΕΜ",1,"LVM",1,"1LE16012AA421GB4"]
["1LE1601-2AA42-2JC4","SIMOTICS SD MOTOR TYPE: 1CV2204A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 200L, * 30kW (50 Hz) 33.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF350 (A400) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",3466,"ΤΕΜ",1,"LVM",1,"1LE16012AA422JC4"]
["1LE1601-2AA53-3JB4","SIMOTICS SD MOTOR TYPE: 1CV2205A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 200L, * 37kW (50 Hz) 41.5kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",4154,"ΤΕΜ",1,"LVM",1,"1LE16012AA533JB4"]
["1LE1601-2AC42-1JB6","SIMOTICS SD MOTOR TYPE: 1CV2204C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 200L, * 18.5 kW (50 Hz) 22 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",3518,"ΤΕΜ",1,"LVM",1,"1LE16012AC421JB6"]
["1LE1601-2BA22-1GB5","SIMOTICS SD MOTOR TYPE: 1CV2222A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 225M * 45kW (50 Hz) 51kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF400 (A450) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",4980,"ΤΕΜ",1,"LVM",1,"1LE16012BA221GB5"]
["1LE1601-2BB00-4AB5","SIMOTICS SD MOTOR TYPE: 1CV2220B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 225S * 37kW (50 Hz) 42.5kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",3817,"ΤΕΜ",1,"LVM",1,"1LE16012BB004AB5"]
["1LE1601-2BB23-3GB5","SIMOTICS SD MOTOR TYPE: 1CV2222B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 225M * 45kW (50 Hz) 52kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF400 (A450) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",4728,"ΤΕΜ",1,"LVM",1,"1LE16012BB233GB5"]
["1LE1601-2BC22-2GC4","SIMOTICS SD MOTOR TYPE: 1CV2222C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 225M * 30kW (50 Hz) 36 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF400 (A450) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",5029,"ΤΕΜ",1,"LVM",1,"1LE16012BC222GC4"]
["1LE1601-2CB22-2GB4","SIMOTICS SD MOTOR TYPE: 1CV2252B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 250M * 55kW (50 Hz) 63kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",5300,"ΤΕΜ",1,"LVM",1,"1LE16012CB222GB4"]
["1LE1601-2CB23-3JB4","SIMOTICS SD MOTOR TYPE: 1CV2252B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 250M * 55kW (50 Hz) 63kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",5495,"ΤΕΜ",1,"LVM",1,"1LE16012CB233JB4"]
["1LE1601-2DA20-4JB6","SIMOTICS SD MOTOR TYPE: 1CV2282A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 280M * 90kW (50 Hz) 101kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",9034,"ΤΕΜ",1,"LVM",1,"1LE16012DA204JB6"]
["1LE1601-2DB02-1AB4","SIMOTICS SD MOTOR TYPE: 1CV2280B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 280S, * 75kW (50 Hz) 86kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",6602,"ΤΕΜ",1,"LVM",1,"1LE16012DB021AB4"]
["1LE1601-2DB20-4JB4","SIMOTICS SD MOTOR TYPE: 1CV2282B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 280M * 90kW (50 Hz) 104kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",8042,"ΤΕΜ",1,"LVM",1,"1LE16012DB204JB4"]
["1LE1601-2DC02-1GB5","SIMOTICS SD MOTOR TYPE: 1CV2280C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 280S, * 45kW (50 Hz) 54kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",7234,"ΤΕΜ",1,"LVM",1,"1LE16012DC021GB5"]
["1LE1601-2DC22-2GC4","SIMOTICS SD MOTOR TYPE: 1CV2282C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 280M * 55kW (50 Hz) 66kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF500 (A550) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",8241,"ΤΕΜ",1,"LVM",1,"1LE16012DC222GC4"]
["1LE1601-3AA03-4JC4","SIMOTICS SD MOTOR TYPE: 1CV2310A low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 315S, * 110kW (50 Hz) 123kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF600 (A660) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",10786,"ΤΕΜ",1,"LVM",1,"1LE16013AA034JC4"]
["1LE1601-3AA43-4JB4","SIMOTICS SD MOTOR TYPE: 1CV2314A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 315L, * 160kW (50 Hz) 180kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",15288,"ΤΕΜ",1,"LVM",1,"1LE16013AA434JB4"]
["1LE1601-3AB22-1AB6","SIMOTICS SD MOTOR TYPE: 1CV2312B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 315M, * 132kW (50 Hz) 152kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",11847,"ΤΕΜ",1,"LVM",1,"1LE16013AB221AB6"]
["1LE1601-3AB42-2AB4","SIMOTICS SD MOTOR TYPE: 1CV2314B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 315L, * 160kW (50 Hz) 184kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",13566,"ΤΕΜ",1,"LVM",1,"1LE16013AB422AB4"]
["1LE1601-3AB52-1AB5","SIMOTICS SD MOTOR TYPE: 1CV2315B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 315L, * 200kW (50 Hz) 230kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",17559,"ΤΕΜ",1,"LVM",1,"1LE16013AB521AB5"]
["1LE1601-3AC20-4AB6","SIMOTICS SD MOTOR TYPE: 1CV2312C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 315M, * 90kW (50 Hz) 108kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",12052,"ΤΕΜ",1,"LVM",1,"1LE16013AC204AB6"]
["1LE1601-3AC22-2AC4","SIMOTICS SD MOTOR TYPE: 1CV2312C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 315M, * 90kW (50 Hz) 108kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",11920,"ΤΕΜ",1,"LVM",1,"1LE16013AC222AC4"]
["1LE1601-3AC50-4AB4","SIMOTICS SD MOTOR TYPE: 1CV2315C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations to be considered! 6-pole * Size 315L, * 132kW (50 Hz) 158kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",16758,"ΤΕΜ",1,"LVM",1,"1LE16013AC504AB4"]
["1LE1603-1AA43-3AB7","SIMOTICS SD MOTOR TYPE: 1CV3104A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box below",672,"ΤΕΜ",1,"LVM",1,"1LE16031AA433AB7"]
["1LE1603-1BA22-2AB6","SIMOTICS SD MOTOR TYPE: 1CV3112A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",770,"ΤΕΜ",1,"LVM",1,"1LE16031BA222AB6"]
["1LE1603-1CA02-2JC4","SIMOTICS SD MOTOR TYPE: 1CV3130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",1080,"ΤΕΜ",1,"LVM",1,"1LE16031CA022JC4"]
["1LE1603-1CA10-4GB6","SIMOTICS SD MOTOR TYPE: 1CV3131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1263,"ΤΕΜ",1,"LVM",1,"1LE16031CA104GB6"]
["1LE1603-1DA23-3AB5","SIMOTICS SD MOTOR TYPE: 1CV3162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",1695,"ΤΕΜ",1,"LVM",1,"1LE16031DA233AB5"]
["1LE1603-1DA23-3JB7","SIMOTICS SD MOTOR TYPE: 1CV3162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1775,"ΤΕΜ",1,"LVM",1,"1LE16031DA233JB7"]
["1LE1603-1DA33-3JB5","SIMOTICS SD MOTOR TYPE: 1CV3163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",2258,"ΤΕΜ",1,"LVM",1,"1LE16031DA333JB5"]
["1LE1603-1DA43-4GC7","SIMOTICS SD MOTOR TYPE: 1CV3164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",2729,"ΤΕΜ",1,"LVM",1,"1LE16031DA434GC7"]
["1LE1603-1EB43-3AB4","SIMOTICS SD MOTOR TYPE: 1CV3184B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 4-pole * Size 180L, * 22kW (50 Hz) 25.3kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2646,"ΤΕΜ",1,"LVM",1,"1LE16031EB433AB4"]
["1LE1603-1EC43-3GB6","SIMOTICS SD MOTOR TYPE: 1CV3184C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 180L, * 15kW (50 Hz) 18kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",3082,"ΤΕΜ",1,"LVM",1,"1LE16031EC433GB6"]
["1LE1603-2AB53-4AB6","SIMOTICS SD MOTOR TYPE: 1CV3205B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 200L, * 30kW (50 Hz) 34.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",3536,"ΤΕΜ",1,"LVM",1,"1LE16032AB534AB6"]
["1LE1603-2AC52-2GB5","SIMOTICS SD MOTOR TYPE: 1CV3205C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 200L, * 22kW (50 Hz) 26.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",4226,"ΤΕΜ",1,"LVM",1,"1LE16032AC522GB5"]
["1LE1603-2AC53-4JC6","SIMOTICS SD MOTOR TYPE: 1CV3205C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 200L, * 22kW (50 Hz) 26.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF350 (A400) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",4443,"ΤΕΜ",1,"LVM",1,"1LE16032AC534JC6"]
["1LE1603-2BC22-1AB4","SIMOTICS SD MOTOR TYPE: 1CV3222C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 225M * 30kW (50 Hz) 36 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",5005,"ΤΕΜ",1,"LVM",1,"1LE16032BC221AB4"]
["1LE1603-2CB23-4AC4","SIMOTICS SD MOTOR TYPE: 1CV3252B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 250M * 55kW (50 Hz) 63kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",5817,"ΤΕΜ",1,"LVM",1,"1LE16032CB234AC4"]
["1LE1603-2CC23-3AB4","SIMOTICS SD MOTOR TYPE: 1CV3252C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 250M * 37kW (50 Hz) 44.5kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",6110,"ΤΕΜ",1,"LVM",1,"1LE16032CC233AB4"]
["1LE1603-2DB02-1GB6","SIMOTICS SD MOTOR TYPE: 1CV3280B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 280S, * 75kW (50 Hz) 86kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",7696,"ΤΕΜ",1,"LVM",1,"1LE16032DB021GB6"]
["1LE1603-2DB23-4AB6","SIMOTICS SD MOTOR TYPE: 1CV3282B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 280M * 90kW (50 Hz) 104kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",8511,"ΤΕΜ",1,"LVM",1,"1LE16032DB234AB6"]
["1LE1603-2DC03-4JC5","SIMOTICS SD MOTOR TYPE: 1CV3280C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 280S, * 45kW (50 Hz) 54kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF500 (A550) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",7891,"ΤΕΜ",1,"LVM",1,"1LE16032DC034JC5"]
["1LE1603-3AB03-3AB5","SIMOTICS SD MOTOR TYPE: 1CV3310B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 4-pole * Size 315S, * 110kW (50 Hz) 127kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",10671,"ΤΕΜ",1,"LVM",1,"1LE16033AB033AB5"]
["1LE1603-3AB42-2AC4","SIMOTICS SD MOTOR TYPE: 1CV3314B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 4-pole * Size 315L, * 160kW (50 Hz) 184kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",14776,"ΤΕΜ",1,"LVM",1,"1LE16033AB422AC4"]
["1LE1603-3AB52-2AC4","SIMOTICS SD MOTOR TYPE: 1CV3315B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 315L, * 200kW (50 Hz) 230kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",18304,"ΤΕΜ",1,"LVM",1,"1LE16033AB522AC4"]
["1LE1603-3AC02-2JB6","SIMOTICS SD MOTOR TYPE: 1CV3310C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 6-pole * Size 315S, * 75kW (50 Hz) 90 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",11968,"ΤΕΜ",1,"LVM",1,"1LE16033AC022JB6"]
["1LE1603-3AC22-2AB5","SIMOTICS SD MOTOR TYPE: 1CV3312C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 315M, * 90kW (50 Hz) 108kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",12850,"ΤΕΜ",1,"LVM",1,"1LE16033AC222AB5"]
["1LE1603-3AC43-3JB5","SIMOTICS SD MOTOR TYPE: 1CV3314C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 315L, * 110kW (50 Hz) 132 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",16047,"ΤΕΜ",1,"LVM",1,"1LE16033AC433JB5"]
["1LE1002-0BA22-2NA4","SIMOTICS GP Motor type: 1AV1062A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) aluminum housing Standard efficiency IE1, 2-pole * Size 63M * 0.18kW (50 Hz) 0.21kW(60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 34, standard flange: FT75 (C90) Without motor protection Terminal box at top",153,"ΤΕΜ",1,"LVM",1,"1LE10020BA222NA4"]
["1LE1003-1BA22-2KB4","SIMOTICS GP MOTOR TYPE: 1AV3112A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 14, Standard flange: FT130 (C160) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",681,"ΤΕΜ",1,"LVM",1,"1LE10031BA222KB4"]
["1LE1001-0DB20-2FA4","SIMOTICS GP Motor type: 1AV2082B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency 4-pole * Size 80M * 0.55kW (50 Hz) 60Hz: IEC 60034-30 0.63kW 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF165 (A200) without motor protection Terminal box at top",243,"ΤΕΜ",1,"LVM",1,"1LE10010DB202FA4"]
["1LE1001-0EA41-7FA4","SIMOTICS GP Motor type: 1AV2094A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 90L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 60 Hz 220 VD/380 VY IM B 5, flange: FF165 (A200) without motor protection Terminal box at top",422,"ΤΕΜ",1,"LVM",1,"1LE10010EA417FA4"]
["1LE1001-1AA42-2LA4","SIMOTICS GP Motor type: 1AV2104A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 kW (60Hz), 50 Hz power 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 19, Standard flange: FT130 (C160) without motor protection Terminal box at top",476,"ΤΕΜ",1,"LVM",1,"1LE10011AA422LA4"]
["1LE1001-1BC21-7JA4","SIMOTICS GP Motor type: 1AV2112C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 112M, * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 60 Hz 220 VD/380 VY IM B 35 * Flange: FF215 (A250) without motor protection Terminal box at top",574,"ΤΕΜ",1,"LVM",1,"1LE10011BC217JA4"]
["1LE1001-1CA11-7JA4","SIMOTICS GP Motor type: 1AV2131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 60 Hz 220 VD/380 VY IM B 35 * Flange: FF265 (A300) without motor protection Terminal box at top",925,"ΤΕΜ",1,"LVM",1,"1LE10011CA117JA4"]
["1LE1001-1CC04-0JA4","SIMOTICS GP Motor type: 1AV2130C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 132S, * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 500 VD * IM B 35 * Flange: FF265 (A300) without motor protection Terminal box at top",692,"ΤΕΜ",1,"LVM",1,"1LE10011CC040JA4"]
["1LE1001-1CC23-1JA4","SIMOTICS GP Motor type: 1AV2132C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 132M, * 4kW (50 Hz) 4.6 kW (60 Hz) 3 AC 60Hz 400VD/690VY IM B 35 * Flange: FF265 (A300) without motor protection Terminal box at top",874,"ΤΕΜ",1,"LVM",1,"1LE10011CC231JA4"]
["1LE1001-1DA21-7FA4","SIMOTICS GP Motor type: 1AV2162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 60 Hz 220 VD/380 VY IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",1270,"ΤΕΜ",1,"LVM",1,"1LE10011DA217FA4"]
["1LE1001-1DA34-0JA4","SIMOTICS GP Motor type: 1AV2163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 500 VD * IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",1588,"ΤΕΜ",1,"LVM",1,"1LE10011DA340JA4"]
["1LE1001-1DB24-0FA4","SIMOTICS GP Motor type: 1AV2162B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 500 VD * IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",1256,"ΤΕΜ",1,"LVM",1,"1LE10011DB240FA4"]
["1LE1001-1DC22-3FA4","SIMOTICS GP Motor type: 1AV2162C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 6-pole * Size 160M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 240 VD/415 VY 3 AC 60 Hz 480 VY IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",1358,"ΤΕΜ",1,"LVM",1,"1LE10011DC223FA4"]
["1LE1001-1DD32-3AA4","SIMOTICS GP Motor type: 1AV2163D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency, 8-pole * Size 160M, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 240 VD/415 VY 3 AC 60 Hz 480 VY IM B 3, without motor protection Terminal box at top",1631,"ΤΕΜ",1,"LVM",1,"1LE10011DD323AA4"]
["1LE1001-1EA23-5JA4","SIMOTICS GP Motor type: 1AV2182A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 180 * 22kW (50 Hz) 24.5kW (60 Hz) 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2245,"ΤΕΜ",1,"LVM",1,"1LE10011EA235JA4"]
["1LE1001-1EB20-2FA4","SIMOTICS GP Motor type: 1AV2182B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 180 * 18.5kW (50 Hz) 21.3kW (60 Hz) 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",1852,"ΤΕΜ",1,"LVM",1,"1LE10011EB202FA4"]
["1LE1001-1EB42-7AA4","SIMOTICS GP Motor type: 1AV2184B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 180 * 22kW (50 Hz) 25.3kW (60 Hz) 3 AC 50Hz 500VY * 3 AC 60Hz 575VY IM B 3, without motor protection Terminal box at top",2025,"ΤΕΜ",1,"LVM",1,"1LE10011EB427AA4"]
["1LE1001-1EC42-3FA4","SIMOTICS GP Motor type: 1AV2184C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 6-pole * Size 180 * 15kW (50 Hz) 18kW (60 Hz) 3 AC 50 Hz 240 VD/415 VY 3 AC 60 Hz 480 VY IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",2331,"ΤΕΜ",1,"LVM",1,"1LE10011EC423FA4"]
["1LE1001-1EC60-2AA4","SIMOTICS GP Motor type: 1AV2186C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum enclosure increased power High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 6-pole * Size 180 * 18.5kW (50 Hz) 22 kW (60 Hz) 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B 3, without motor protection Terminal box at top",2638,"ΤΕΜ",1,"LVM",1,"1LE10011EC602AA4"]
["1LE1001-1ED43-5AA4","SIMOTICS GP Motor type: 1AV2184D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, 60 Hz, P60: IE1 8-pole * Size 180 * 11kW (50 Hz) 13.2kW (60 Hz) 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 3, without motor protection Terminal box at top",2365,"ΤΕΜ",1,"LVM",1,"1LE10011ED435AA4"]
["1LE1001-2AA46-3JA4","SIMOTICS GP Motor type: 1AV2204A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 200 * 30kW (50 Hz) 33.5kW (60 Hz) 3 AC 60 Hz 230 VDD * 50 Hz 460 VD * 12 main terminals electrical according to NEMA IM B 35 * Flange: FF350 (A400) without motor protection Terminal box at top",2902,"ΤΕΜ",1,"LVM",1,"1LE10012AA463JA4"]
["1LE1001-2AB52-7FA4","SIMOTICS GP Motor type: 1AV2205B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 200 * 30kW (50 Hz) 34.5kW (60 Hz) 3 AC 50Hz 500VY * 3 AC 60Hz 575VY IM B 5, flange: FF350 (A400) without motor protection Terminal box at top",2758,"ΤΕΜ",1,"LVM",1,"1LE10012AB527FA4"]
["1LE1001-2AB62-2AA4","SIMOTICS GP Motor type: 1AV2206B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum enclosure increased power High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 200 * 37kW (50 Hz) 42.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, without motor protection Terminal box at top",3184,"ΤΕΜ",1,"LVM",1,"1LE10012AB622AA4"]
["1LE1001-2AC50-2JA4","SIMOTICS GP Motor type: 1AV2205C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 200 * 22kW (50 Hz) 26.5kW (60 Hz) 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF350 (A400) without motor protection Terminal box at top",3239,"ΤΕΜ",1,"LVM",1,"1LE10012AC502JA4"]
["1LE1001-2AD51-7FA4","SIMOTICS GP Motor type: 1AV2205D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, 8-pole * Size 200 * 15kW (50 Hz) 18kW (60 Hz) 3 AC 60 Hz 220 VD/380 VY IM B 5, flange: FF350 (A400) without motor protection Terminal box at top",3241,"ΤΕΜ",1,"LVM",1,"1LE10012AD517FA4"]
["1LE1003-0DB20-2JA4","SIMOTICS GP MOTOR TYPE: 1AV3082B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing Premium Efficiency, 4-pole * Size 80M * 0.55kW (50 Hz) 0.63kW (60 Hz) 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF165 (A200) WITHOUT MOTOR PROTECTION Terminal box at top",286,"ΤΕΜ",1,"LVM",1,"1LE10030DB202JA4"]
["1LE1003-0DB32-7FA4","SIMOTICS GP MOTOR TYPE: 1AV3083B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 80M * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50Hz 500VY * 3 AC 60Hz 575VY IM B 5, flange: FF165 (A200) WITHOUT MOTOR PROTECTION Terminal box at top",310,"ΤΕΜ",1,"LVM",1,"1LE10030DB327FA4"]
["1LE1003-0EB42-3JA4","SIMOTICS GP MOTOR TYPE: 1AV3094B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 90L * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 240 VD/415 VY 3 AC 60 Hz 480 VY IM B 35 * Flange: FF165 (A200) WITHOUT MOTOR PROTECTION Terminal box at top",449,"ΤΕΜ",1,"LVM",1,"1LE10030EB423JA4"]
["1LE1003-1AA42-3FA4","SIMOTICS GP MOTOR TYPE: 1AV3104A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 240 VD/415 VY 3 AC 60 Hz 480 VY IM B 5, flange: FF215 (A250) Without motor protection Terminal box at top",553,"ΤΕΜ",1,"LVM",1,"1LE10031AA423FA4"]
["1LE1003-1AB52-3AA4","SIMOTICS GP MOTOR TYPE: 1AV3105B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 240 VD/415 VY 3 AC 60 Hz 480 VY IM B3 Without motor protection Terminal box at top",548,"ΤΕΜ",1,"LVM",1,"1LE10031AB523AA4"]
["1LE1003-1BB22-7FA4","SIMOTICS GP MOTOR TYPE: 1AV3112B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50Hz 500VY * 3 AC 60Hz 575VY IM B 5, flange: FF215 (A250) Without motor protection Terminal box at top",681,"ΤΕΜ",1,"LVM",1,"1LE10031BB227FA4"]
["1LE1003-1CA13-5AA4","SIMOTICS GP MOTOR TYPE: 1AV3131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B3 Without motor protection Terminal box at top",972,"ΤΕΜ",1,"LVM",1,"1LE10031CA135AA4"]
["1LE1003-1CB60-2JA4","SIMOTICS GP MOTOR TYPE: 1AV3136B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum enclosure increased power Premium Efficiency IE3, 4-pole * Size 132M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF265 (A300) without motor protection Terminal box at top",1389,"ΤΕΜ",1,"LVM",1,"1LE10031CB602JA4"]
["1LE1003-1CC31-8FA4","SIMOTICS GP MOTOR TYPE: 1AV3133C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 132M, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 60 Hz 230 VD/400 VY IM B 5, flange: FF265 (A300) without motor protection Terminal box at top",1196,"ΤΕΜ",1,"LVM",1,"1LE10031CC318FA4"]
["1LE1003-1CD23-1JA4","SIMOTICS GP MOTOR TYPE: 1AV3132D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 132M, * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 60Hz 400VD/690VY IM B 35 * Flange: FF265 (A300) without motor protection Terminal box at top",1408,"ΤΕΜ",1,"LVM",1,"1LE10031CD231JA4"]
["1LE1003-1DA34-0JA4","SIMOTICS GP MOTOR TYPE: 1AV3163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 500 VD * IM B 35, flange: FF300 (A350) Without motor protection Terminal box at top",1785,"ΤΕΜ",1,"LVM",1,"1LE10031DA340JA4"]
["1LE1003-1DA60-2JA4","SIMOTICS GP MOTOR TYPE: 1AV3166A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum enclosure increased power Premium Efficiency IE3, 2-pole * Size 160L, * 22kW (50 Hz) 25.3kW (60 Hz) 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2390,"ΤΕΜ",1,"LVM",1,"1LE10031DA602JA4"]
["1LE1003-1DB61-7JA4","SIMOTICS GP MOTOR TYPE: 1AV3166B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum enclosure increased power Premium Efficiency IE3, 4-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 60 Hz 220 VD/380 VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2080,"ΤΕΜ",1,"LVM",1,"1LE10031DB617JA4"]
["1LE1003-1DC42-7JA4","SIMOTICS GP MOTOR TYPE: 1AV3164C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 160L, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50Hz 500VY * 3 AC 60Hz 575VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2012,"ΤΕΜ",1,"LVM",1,"1LE10031DC427JA4"]
["1LE1003-1EA21-8JA4","SIMOTICS GP MOTOR TYPE: 1AV3182A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 180 * 22kW (50 Hz) 24.5kW (60 Hz) 3 AC 60 Hz 230 VD/400 VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2455,"ΤΕΜ",1,"LVM",1,"1LE10031EA218JA4"]
["1LE1003-1EB43-5FA4","SIMOTICS GP MOTOR TYPE: 1AV3184B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 4-pole * Size 180 * 22kW (50 Hz) 25.3kW (60 Hz) 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",2394,"ΤΕΜ",1,"LVM",1,"1LE10031EB435FA4"]
["1LE1003-1EC40-2JA4","SIMOTICS GP MOTOR TYPE: 1AV3184C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 180 * 15kW (50 Hz) 18kW (60 Hz) 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2518,"ΤΕΜ",1,"LVM",1,"1LE10031EC402JA4"]
["1LE1003-1ED43-1FA4","SIMOTICS GP MOTOR TYPE: 1AV3184D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 8-pole * Size 180 * 11kW (50 Hz) 13.2kW (60 Hz) 3 AC 60Hz 400VD/690VY IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",2990,"ΤΕΜ",1,"LVM",1,"1LE10031ED431FA4"]
["1LE1003-2AA56-3JA4","SIMOTICS GP MOTOR TYPE: 1AV3205A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 200 * 37kW (50 Hz) 41.5kW (60 Hz) 3 AC 60 Hz 230 VDD * 50 Hz 460 VD * 12 main terminals electrical according to NEMA IM B 35 * Flange: FF350 (A400) without motor protection Terminal box at top",3927,"ΤΕΜ",1,"LVM",1,"1LE10032AA563JA4"]
["1LE1003-2AB63-5JA4","SIMOTICS GP MOTOR TYPE: 1AV3206B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum enclosure increased power Premium Efficiency IE3, 4-pole * Size 200 * 37kW (50 Hz) 42.5kW (60 Hz) 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 35 * Flange: FF350 (A400) without motor protection Terminal box at top",3667,"ΤΕΜ",1,"LVM",1,"1LE10032AB635JA4"]
["1LE1003-2AC42-2FA4","SIMOTICS GP MOTOR TYPE: 1AV3204C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 200 * 18.5kW (50 Hz) 22 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF350 (A400) without motor protection Terminal box at top",3048,"ΤΕΜ",1,"LVM",1,"1LE10032AC422FA4"]
["1LE1003-2AC62-1JA4","SIMOTICS GP MOTOR TYPE: 1AV3206C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum enclosure increased power Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 200 * 30kW (50 Hz) 36 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF350 (A400) without motor protection Terminal box at top",4645,"ΤΕΜ",1,"LVM",1,"1LE10032AC621JA4"]
["1LE1004-1CA13-1FA4","SIMOTICS GP MOTOR TYPE: 1AV4131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 60Hz 400VD/690VY IM B 5, flange: FF265 (A300) without motor protection Terminal box at top",1225,"ΤΕΜ",1,"LVM",1,"1LE10041CA131FA4"]
["1LE1004-1CB23-0FA4","SIMOTICS GP MOTOR TYPE: 1AV4132B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 132M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 60 Hz 380 VD/660 VY IM B 5, flange: FF265 (A300) without motor protection Terminal box at top",1317,"ΤΕΜ",1,"LVM",1,"1LE10041CB230FA4"]
["1LE1004-1DB42-7FA4","SIMOTICS GP MOTOR TYPE: 1AV4164B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 160L, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50Hz 500VY * 3 AC 60Hz 575VY IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",2159,"ΤΕΜ",1,"LVM",1,"1LE10041DB427FA4"]
["1LE1004-1EB23-0FA4","SIMOTICS GP MOTOR TYPE: 1AV4182B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4 4-pole * Size 180M, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 60 Hz 380 VD/660 VY IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",2499,"ΤΕΜ",1,"LVM",1,"1LE10041EB230FA4"]
["1LE1004-1EB46-0AA4","SIMOTICS GP MOTOR TYPE: 1AV4184B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 4-pole * Size 180L, * 22kW (50 Hz) 25.3kW (60 Hz) 3 AC 60 Hz 230 VYY * 50 Hz 460 VY * 9 main terminals electrical according to NEMA IM B 3, without motor protection Terminal box at top",2743,"ΤΕΜ",1,"LVM",1,"1LE10041EB460AA4"]
["1LE1004-2AA50-2AA4","SIMOTICS GP MOTOR TYPE: 1AV4205A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 200L, * 37kW (50 Hz) 41.5kW (60 Hz) 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B 3, without motor protection Terminal box at top",4452,"ΤΕΜ",1,"LVM",1,"1LE10042AA502AA4"]
["1LE1011-1AL53-4FA4","SIMOTICS GP MOTOR TYPE: 1AV1105L Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing Double pole-changing * One winding in Dahlander circuit 8/4-pole*Size 100L* 0.9/1.5kW (50 Hz) 3 AC 50Hz 400V IM B 5, flange: FF215 (A250) without motor protection Terminal box at top",447,"ΤΕΜ",1,"LVM",1,"1LE10111AL534FA4"]
["1LE1501-0CC23-4AA4","SIMOTICS SD MOTOR TYPE: 1CV2072C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 6-pole * Size 71M * 0.18kW (50 Hz) 0.21kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box at top",217,"ΤΕΜ",1,"LVM",1,"1LE15010CC234AA4"]
["1LE1501-0CD23-0JA4","SIMOTICS SD MOTOR TYPE: 1CV2072D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 8-pole * Size 71M * 0.09kW (50 Hz) 3 AC 60 Hz 380 VD/660 VY IM B 35 * Flange: FF130 (A160) without motor protection Terminal box at top",289,"ΤΕΜ",1,"LVM",1,"1LE15010CD230JA4"]
["1LE1501-0DB31-7AA4","SIMOTICS SD MOTOR TYPE: 1CV2083B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) High Efficiency IE2, 4-pole * Size 80M * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 60 Hz 220 VD/380 VY IM B 3, without motor protection Terminal box at top",311,"ΤΕΜ",1,"LVM",1,"1LE15010DB317AA4"]
["1LE1501-0EA02-2FA4","SIMOTICS SD MOTOR TYPE: 1CV2090A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) High Efficiency IE2, 2-pole * Size 90S * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF165 (A200) without motor protection Terminal box at top",388,"ΤΕΜ",1,"LVM",1,"1LE15010EA022FA4"]
["1LE1501-0EB40-4JA4","SIMOTICS SD MOTOR TYPE: 1CV2094B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) High Efficiency IE2, 4-pole * Size 90L * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF165 (A200) without motor protection Terminal box at top",422,"ΤΕΜ",1,"LVM",1,"1LE15010EB404JA4"]
["1LE1501-0EC00-2JA4","SIMOTICS SD MOTOR TYPE: 1CV2090C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) High Efficiency IE2, 6-pole * Size 90S * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF165 (A200) without motor protection Terminal box at top",371,"ΤΕΜ",1,"LVM",1,"1LE15010EC002JA4"]
["1LE1501-1AB42-7JA4","SIMOTICS SD MOTOR TYPE: 1CV2104B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) High Efficiency IE2, 4-pole * Size 100L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 500 VY 3 AC 60Hz 575VY IM B 35 * Flange: FF215 (A250) without motor protection Terminal box at top",475,"ΤΕΜ",1,"LVM",1,"1LE15011AB427JA4"]
["1LE1501-1AC42-7FA4","SIMOTICS SD MOTOR TYPE: 1CV2104C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) High Efficiency IE2, 6-pole * Size 100L * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 500 VY 3 AC 60Hz 575VY IM B 5, flange: FF215 (A250) without motor protection Terminal box at top",467,"ΤΕΜ",1,"LVM",1,"1LE15011AC427FA4"]
["1LE1501-1BB23-3JA4","SIMOTICS SD MOTOR TYPE: 1CV2112B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) High Efficiency IE2, 4-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF215 (A250) without motor protection Terminal box at top",687,"ΤΕΜ",1,"LVM",1,"1LE15011BB233JA4"]
["1LE1501-1BC22-1AA4","SIMOTICS SD MOTOR TYPE: 1CV2112C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) High Efficiency IE2, 6-pole * Size 112M, * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, without motor protection Terminal box at top",578,"ΤΕΜ",1,"LVM",1,"1LE15011BC221AA4"]
["1LE1501-1CA13-1AA4","SIMOTICS SD MOTOR TYPE: 1CV2131A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 132S, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 60Hz 400VD/690VY IM B 3, without motor protection Terminal box at top",943,"ΤΕΜ",1,"LVM",1,"1LE15011CA131AA4"]
["1LE1501-1CB03-0FA4","SIMOTICS SD MOTOR TYPE: 1CV2130B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) High Efficiency IE2, 4-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 60 Hz 380 VD/660 VY IM B 5, flange: FF265 (A300) without motor protection Terminal box at top",864,"ΤΕΜ",1,"LVM",1,"1LE15011CB030FA4"]
["1LE1501-1CC20-4FA4","SIMOTICS SD MOTOR TYPE: 1CV2132C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) High Efficiency IE2, 6-pole * Size 132M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF265 (A300) without motor protection Terminal box at top",900,"ΤΕΜ",1,"LVM",1,"1LE15011CC204FA4"]
["1LE1501-1CC23-4FA4","SIMOTICS SD MOTOR TYPE: 1CV2132C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) High Efficiency IE2, 6-pole * Size 132M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF265 (A300) without motor protection Terminal box at top",900,"ΤΕΜ",1,"LVM",1,"1LE15011CC234FA4"]
["1LE1501-1CD21-8FA4","SIMOTICS SD MOTOR TYPE: 1CV2132D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 8-pole * Size 132M, * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 60 Hz 230 VD/400 VY IM B 5, flange: FF265 (A300) without motor protection Terminal box at top",1233,"ΤΕΜ",1,"LVM",1,"1LE15011CD218FA4"]
["1LE1501-1DA24-0JA4","SIMOTICS SD MOTOR TYPE: 1CV2162A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 500 VD 3 AC 60 Hz 575 VD IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",1336,"ΤΕΜ",1,"LVM",1,"1LE15011DA240JA4"]
["1LE1501-1DA62-7JA4","SIMOTICS SD MOTOR TYPE: 1CV2166A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Cast iron frame, increased power Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations to be considered! 2-pole * Size 160L, * 22kW (50 Hz) 24.5kW (60 Hz) 3 AC 50 Hz 500 VY 3 AC 60Hz 575VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2386,"ΤΕΜ",1,"LVM",1,"1LE15011DA627JA4"]
["1LE1501-1DB22-7JA4","SIMOTICS SD MOTOR TYPE: 1CV2162B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 500 VY 3 AC 60Hz 575VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",1361,"ΤΕΜ",1,"LVM",1,"1LE15011DB227JA4"]
["1LE1501-1DC23-4AA4","SIMOTICS SD MOTOR TYPE: 1CV2162C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 6-pole * Size 160M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box at top",1344,"ΤΕΜ",1,"LVM",1,"1LE15011DC234AA4"]
["1LE1501-1DD23-4JA4","SIMOTICS SD MOTOR TYPE: 1CV2162D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 8-pole * Size 160M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",1483,"ΤΕΜ",1,"LVM",1,"1LE15011DD234JA4"]
["1LE1501-1DD43-5JA4","SIMOTICS SD MOTOR TYPE: 1CV2164D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 8-pole * Size 160L, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2202,"ΤΕΜ",1,"LVM",1,"1LE15011DD435JA4"]
["1LE1501-1EA23-0JA4","SIMOTICS SD MOTOR TYPE: 1CV2182A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 180M, * 22kW (50 Hz) 24.5kW (60 Hz) 3 AC 60 Hz 380 VD/660 VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2375,"ΤΕΜ",1,"LVM",1,"1LE15011EA230JA4"]
["1LE1501-1EB43-1JA4","SIMOTICS SD MOTOR TYPE: 1CV2184B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 180L, * 22kW (50 Hz) 25.3kW (60 Hz) 3 AC 60Hz 400VD/690VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2346,"ΤΕΜ",1,"LVM",1,"1LE15011EB431JA4"]
["1LE1501-1EC60-2AA4","SIMOTICS SD MOTOR TYPE: 1CV2186C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Cast iron frame, increased power Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 6-pole * Size 180L, * 18.5 kW (50 Hz) 22 kW (60 Hz) 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B 3, without motor protection Terminal box at top",2861,"ΤΕΜ",1,"LVM",1,"1LE15011EC602AA4"]
["1LE1501-1ED42-7AA4","SIMOTICS SD MOTOR TYPE: 1CV2184D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 8-pole * Size 180L, * 11kW (50 Hz) 13.2kW (60 Hz) 3 AC 50 Hz 500 VY 3 AC 60Hz 575VY IM B 3, without motor protection Terminal box at top",2449,"ΤΕΜ",1,"LVM",1,"1LE15011ED427AA4"]
["1LE1501-2AB54-0FA4","SIMOTICS SD MOTOR TYPE: 1CV2205B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 200L, * 30kW (50 Hz) 34.5kW (60 Hz) 3 AC 50 Hz 500 VD 3 AC 60 Hz 575 VD IM B 5, flange: FF350 (A400) without motor protection Terminal box at top",2926,"ΤΕΜ",1,"LVM",1,"1LE15012AB540FA4"]
["1LE1501-2AC44-0JA4","SIMOTICS SD MOTOR TYPE: 1CV2204C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 200L, * 18.5 kW (50 Hz) 22 kW (60 Hz) 3 AC 50 Hz 500 VD 3 AC 60 Hz 575 VD IM B 35 * Flange: FF350 (A400) without motor protection Terminal box at top",2982,"ΤΕΜ",1,"LVM",1,"1LE15012AC440JA4"]
["1LE1501-2AD51-7FA4","SIMOTICS SD MOTOR TYPE: 1CV2205D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 8-pole * Size 200L, * 15kW (50 Hz) 18kW (60 Hz) 3 AC 60 Hz 220 VD/380 VY IM B 5, flange: FF350 (A400) without motor protection Terminal box at top",3438,"ΤΕΜ",1,"LVM",1,"1LE15012AD517FA4"]
["1LE1501-2BA63-4JA4","SIMOTICS SD MOTOR TYPE: 1CV2226A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Cast iron frame, increased power Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 225M * 55kW (50 Hz) 62kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF400 (A450) without motor protection Terminal box at top",5135,"ΤΕΜ",1,"LVM",1,"1LE15012BA634JA4"]
["1LE1501-2BB21-8FA4","SIMOTICS SD MOTOR TYPE: 1CV2222B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 225M * 45kW (50 Hz) 52kW (60 Hz) 3 AC 60 Hz 230 VD/400 VY IM B 5, flange: FF400 (A450) without motor protection Terminal box at top",4124,"ΤΕΜ",1,"LVM",1,"1LE15012BB218FA4"]
["1LE1501-2BC23-5FA4","SIMOTICS SD MOTOR TYPE: 1CV2222C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 225M * 30kW (50 Hz) 36 kW (60 Hz) 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 5, flange: FF400 (A450) without motor protection Terminal box at top",4468,"ΤΕΜ",1,"LVM",1,"1LE15012BC235FA4"]
["1LE1501-2BD02-7FA4","SIMOTICS SD MOTOR TYPE: 1CV2220D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 8-pole * Size 225S * 18.5kW (50 Hz) 22 kW (60 Hz) 3 AC 50 Hz 500 VY 3 AC 60Hz 575VY IM B 5, flange: FF400 (A450) without motor protection Terminal box at top",3975,"ΤΕΜ",1,"LVM",1,"1LE15012BD027FA4"]
["1LE1501-2CB60-4FA4","SIMOTICS SD MOTOR TYPE: 1CV2256B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Cast iron frame, increased power Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 250M * 75kW (50 Hz) 86kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF500 (A550) without motor protection Terminal box at top",6639,"ΤΕΜ",1,"LVM",1,"1LE15012CB604FA4"]
["1LE1501-2CC64-0AA4","SIMOTICS SD MOTOR TYPE: 1CV2256C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Cast iron frame, increased power Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 250M * 45kW (50 Hz) 54kW (60 Hz) 3 AC 50 Hz 500 VD 3 AC 60 Hz 575 VD IM B3 without motor protection Terminal box at top",6384,"ΤΕΜ",1,"LVM",1,"1LE15012CC640AA4"]
["1LE1501-2DA03-5JA4","SIMOTICS SD MOTOR TYPE: 1CV2280A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 280S, * 75kW (50 Hz) 84kW (60 Hz) 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 35 * Flange: FF500 (A550) without motor protection Terminal box at top",7209,"ΤΕΜ",1,"LVM",1,"1LE15012DA035JA4"]
["1LE1501-2DB20-2FA4","SIMOTICS SD MOTOR TYPE: 1CV2282B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 280M * 90kW (50 Hz) 104kW (60 Hz) 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF500 (A550) without motor protection Terminal box at top",7660,"ΤΕΜ",1,"LVM",1,"1LE15012DB202FA4"]
["1LE1501-2DB61-7AA4","SIMOTICS SD MOTOR TYPE: 1CV2286B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Cast iron frame, increased power Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 280M * 110kW (50 Hz) 127kW (60 Hz) 3 AC 60 Hz 220 VD/380 VY IM B 3, without motor protection Terminal box at top",9500,"ΤΕΜ",1,"LVM",1,"1LE15012DB617AA4"]
["1LE1501-2DC04-0AA4","SIMOTICS SD MOTOR TYPE: 1CV2280C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 280S, * 45kW (50 Hz) 54kW (60 Hz) 3 AC 50 Hz 500 VD 3 AC 60 Hz 575 VD IM B 3, without motor protection Terminal box at top",6216,"ΤΕΜ",1,"LVM",1,"1LE15012DC040AA4"]
["1LE1501-2DD01-8AA4","SIMOTICS SD MOTOR TYPE: 1CV2280D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 8-pole * Size 280S, * 37kW (50 Hz) 44.5kW (60 Hz) 3 AC 60 Hz 230 VD/400 VY IM B 3, without motor protection Terminal box at top",6854,"ΤΕΜ",1,"LVM",1,"1LE15012DD018AA4"]
["1LE1501-3AA03-0JA4","SIMOTICS SD MOTOR TYPE: 1CV2310A low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 2-pole * Size 315S, * 110kW (50 Hz) 123kW (60 Hz) 3 AC 60 Hz 380 VD/660 VY IM B 35 * Flange: FF600 (A660) without motor protection Terminal box at top",9971,"ΤΕΜ",1,"LVM",1,"1LE15013AA030JA4"]
["1LE1501-3AB04-0AA4","SIMOTICS SD MOTOR TYPE: 1CV2310B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 315S, * 110kW (50 Hz) 127kW (60 Hz) 3 AC 50 Hz 500 VD 3 AC 60 Hz 575 VD IM B 3, without motor protection Terminal box at top",9198,"ΤΕΜ",1,"LVM",1,"1LE15013AB040AA4"]
["1LE1501-3AC03-5JA4","SIMOTICS SD MOTOR TYPE: 1CV2310C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 60 Hz, P60: IE1 In EEA: Minimum efficiency according to applicable statutory regulations to be considered 6-pole * Size 315S, * 75kW (50 Hz) 90 kW (60 Hz) 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 35 * Flange: FF600 (A660) without motor protection Terminal box at top",10758,"ΤΕΜ",1,"LVM",1,"1LE15013AC035JA4"]
["1LE1501-3AC62-7JA4","SIMOTICS SD MOTOR TYPE: 1CV2316C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations to be considered! 6-pole * Size 315L, * 160kW (50 Hz) 192kW (60 Hz) 3 AC 50 Hz 500 VY 3 AC 60Hz 575VY IM B 35 * Flange: FF600 (A660) without motor protection Terminal box at top",20160,"ΤΕΜ",1,"LVM",1,"1LE15013AC627JA4"]
["1LE1501-3AD20-4JA4","SIMOTICS SD MOTOR TYPE: 1CV2312D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 8-pole * Size 315M, * 75kW (50 Hz) 90 kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF600 (A660) without motor protection Terminal box at top",13482,"ΤΕΜ",1,"LVM",1,"1LE15013AD204JA4"]
["1LE1501-3AD63-3JA4","SIMOTICS SD MOTOR TYPE: 1CV2316D Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Cast iron frame, increased power Basic line High Efficiency IE2, 8-pole * Size 315L, * 132kW (50 Hz) 158kW (60 Hz) 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF600 (A660) without motor protection Terminal box at top",21510,"ΤΕΜ",1,"LVM",1,"1LE15013AD633JA4"]
["1LE1503-0CB30-2AA4","SIMOTICS SD MOTOR TYPE: 1CV3073B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 4-pole * Size 71M * 0.37kW (50 Hz) 0.43kW (60 Hz) 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B 3, without motor protection Terminal box at top",315,"ΤΕΜ",1,"LVM",1,"1LE15030CB302AA4"]
["1LE1503-0CC23-5AA4","SIMOTICS SD MOTOR TYPE: 1CV3072C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 6-pole * Size 71M * 0.18kW (50 Hz) 0.21kW (60 Hz) 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 3, without motor protection Terminal box at top",286,"ΤΕΜ",1,"LVM",1,"1LE15030CC235AA4"]
["1LE1503-0CC32-2FA4","SIMOTICS SD MOTOR TYPE: 1CV3073C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 6-pole * Size 71M * 0.25kW (50 Hz) 0.29kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF130 (A160) without motor protection Terminal box at top",343,"ΤΕΜ",1,"LVM",1,"1LE15030CC322FA4"]
["1LE1503-0DB23-5JA4","SIMOTICS SD MOTOR TYPE: 1CV3082B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 4-pole * Size 80M * 0.55kW (50 Hz) 0.63kW (60 Hz) 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 35 * Flange: FF165 (A200) without motor protection Terminal box at top",378,"ΤΕΜ",1,"LVM",1,"1LE15030DB235JA4"]
["1LE1503-0DC22-2FA4","SIMOTICS SD MOTOR TYPE: 1CV3082C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 6-pole * Size 80M * 0.37kW (50 Hz) 0.43kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF165 (A200) without motor protection Terminal box at top",352,"ΤΕΜ",1,"LVM",1,"1LE15030DC222FA4"]
["1LE1503-0EA03-0JA4","SIMOTICS SD MOTOR TYPE: 1CV3090A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 90S * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 60 Hz 380 VD/660 VY IM B 35 * Flange: FF165 (A200) without motor protection Terminal box at top",497,"ΤΕΜ",1,"LVM",1,"1LE15030EA030JA4"]
["1LE1503-0EC01-8AA4","SIMOTICS SD MOTOR TYPE: 1CV3090C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 6-pole * Size 90S * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 60 Hz 230 VD/400 VY IM B 3, without motor protection Terminal box at top",447,"ΤΕΜ",1,"LVM",1,"1LE15030EC018AA4"]
["1LE1503-1AA40-2FA4","SIMOTICS SD MOTOR TYPE: 1CV3104A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF215 (A250) without motor protection Terminal box at top",581,"ΤΕΜ",1,"LVM",1,"1LE15031AA402FA4"]
["1LE1503-1AB53-0AA4","SIMOTICS SD MOTOR TYPE: 1CV3105B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 4-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 60 Hz 380 VD/660 VY IM B 3, without motor protection Terminal box at top",594,"ΤΕΜ",1,"LVM",1,"1LE15031AB530AA4"]
["1LE1503-1AC41-8JA4","SIMOTICS SD MOTOR TYPE: 1CV3104C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 100L * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 60 Hz 230 VD/400 VY IM B 35 * Flange: FF215 (A250) without motor protection Terminal box at top",544,"ΤΕΜ",1,"LVM",1,"1LE15031AC418JA4"]
["1LE1503-1BC21-7JA4","SIMOTICS SD MOTOR TYPE: 1CV3112C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 112M, * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 60 Hz 220 VD/380 VY IM B 35 * Flange: FF215 (A250) without motor protection Terminal box at top",687,"ΤΕΜ",1,"LVM",1,"1LE15031BC217JA4"]
["1LE1503-1CA04-0JA4","SIMOTICS SD MOTOR TYPE: 1CV3130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 500 VD 3 AC 60 Hz 575 VD IM B 35 * Flange: FF265 (A300) without motor protection Terminal box at top",860,"ΤΕΜ",1,"LVM",1,"1LE15031CA040JA4"]
["1LE1503-1CA64-0FA4","SIMOTICS SD MOTOR TYPE: 1CV3136A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Cast iron frame, increased power Basic line Premium Efficiency IE3, 2-pole * Size 132M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 500 VD 3 AC 60 Hz 575 VD IM B 5, flange: FF265 (A300) without motor protection Terminal box at top",1467,"ΤΕΜ",1,"LVM",1,"1LE15031CA640FA4"]
["1LE1503-1CC03-1JA4","SIMOTICS SD MOTOR TYPE: 1CV3130C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 132S, * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 60Hz 400VD/690VY IM B 35 * Flange: FF265 (A300) without motor protection Terminal box at top",874,"ΤΕΜ",1,"LVM",1,"1LE15031CC031JA4"]
["1LE1503-1CC23-5JA4","SIMOTICS SD MOTOR TYPE: 1CV3132C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 132M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 35 * Flange: FF265 (A300) without motor protection Terminal box at top",1042,"ΤΕΜ",1,"LVM",1,"1LE15031CC235JA4"]
["1LE1503-1DA31-8JA4","SIMOTICS SD MOTOR TYPE: 1CV3163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 60 Hz 230 VD/400 VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",1971,"ΤΕΜ",1,"LVM",1,"1LE15031DA318JA4"]
["1LE1503-1DB22-1FA4","SIMOTICS SD MOTOR TYPE: 1CV3162B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 4-pole * Size 160M, * 11kW (50 Hz) 12.6kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",1568,"ΤΕΜ",1,"LVM",1,"1LE15031DB221FA4"]
["1LE1503-1DB60-4JA4","SIMOTICS SD MOTOR TYPE: 1CV3166B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Cast iron frame, increased power Basic line Premium Efficiency IE3, 4-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2163,"ΤΕΜ",1,"LVM",1,"1LE15031DB604JA4"]
["1LE1503-1EA63-1FA4","SIMOTICS SD MOTOR TYPE: 1CV3186A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Cast iron frame, increased power Basic line Premium Efficiency IE3, 2-pole * Size 180L, * 30kW (50 Hz) 33.5kW (60 Hz) 3 AC 60Hz 400VD/690VY IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",3297,"ΤΕΜ",1,"LVM",1,"1LE15031EA631FA4"]
["1LE1503-1EB23-1FA4","SIMOTICS SD MOTOR TYPE: 1CV3182B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 4-pole * Size 180M, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 60Hz 400VD/690VY IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",2217,"ΤΕΜ",1,"LVM",1,"1LE15031EB231FA4"]
["1LE1503-2AA63-1FA4","SIMOTICS SD MOTOR TYPE: 1CV3206A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Cast iron frame, increased power Basic line Premium Efficiency IE3, 2-pole * Size 200L, * 45kW (50 Hz) 51kW (60 Hz) 3 AC 60Hz 400VD/690VY IM B 5, flange: FF350 (A400) without motor protection Terminal box at top",4732,"ΤΕΜ",1,"LVM",1,"1LE15032AA631FA4"]
["1LE1503-2AB60-2AA4","SIMOTICS SD MOTOR TYPE: 1CV3206B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Cast iron frame, increased power Basic line Premium Efficiency IE3, 4-pole * Size 200L, * 37kW (50 Hz) 42.5kW (60 Hz) 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B 3, without motor protection Terminal box at top",3654,"ΤΕΜ",1,"LVM",1,"1LE15032AB602AA4"]
["1LE1503-2BA61-7FA4","SIMOTICS SD MOTOR TYPE: 1CV3226A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Cast iron frame, increased power Basic line Premium Efficiency IE3, 2-pole * Size 225M * 55kW (50 Hz) 62kW (60 Hz) 3 AC 60 Hz 220 VD/380 VY IM B 5, flange: FF400 (A450) without motor protection Terminal box at top",5560,"ΤΕΜ",1,"LVM",1,"1LE15032BA617FA4"]
["1LE1503-2BB24-0FA4","SIMOTICS SD MOTOR TYPE: 1CV3222B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 225M * 45kW (50 Hz) 52kW (60 Hz) 3 AC 50 Hz 500 VD 3 AC 60 Hz 575 VD IM B 5, flange: FF400 (A450) without motor protection Terminal box at top",4332,"ΤΕΜ",1,"LVM",1,"1LE15032BB240FA4"]
["1LE1503-2CA61-8JA4","SIMOTICS SD MOTOR TYPE: 1CV3256A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Cast iron frame, increased power Basic line Premium Efficiency IE3, 2-pole * Size 250M * 75kW (50 Hz) 84kW (60 Hz) 3 AC 60 Hz 230 VD/400 VY IM B 35 * Flange: FF500 (A550) without motor protection Terminal box at top",7595,"ΤΕΜ",1,"LVM",1,"1LE15032CA618JA4"]
["1LE1503-2CB60-4FA4","SIMOTICS SD MOTOR TYPE: 1CV3256B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Cast iron frame, increased power Basic line Premium Efficiency IE3, 4-pole * Size 250M * 75kW (50 Hz) 86kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF500 (A550) without motor protection Terminal box at top",7017,"ΤΕΜ",1,"LVM",1,"1LE15032CB604FA4"]
["1LE1503-2DA63-4JA4","SIMOTICS SD MOTOR TYPE: 1CV3286A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Cast iron frame, increased power Basic line Premium Efficiency IE3, 2-pole * Size 280M * 110kW (50 Hz) 123kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF500 (A550) without motor protection Terminal box at top",10478,"ΤΕΜ",1,"LVM",1,"1LE15032DA634JA4"]
["1LE1503-2DC21-7FA4","SIMOTICS SD MOTOR TYPE: 1CV3282C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 280M * 55kW (50 Hz) 66kW (60 Hz) 3 AC 60 Hz 220 VD/380 VY IM B 5, flange: FF500 (A550) without motor protection Terminal box at top",8340,"ΤΕΜ",1,"LVM",1,"1LE15032DC217FA4"]
["1LE1503-3AA23-5FA4","SIMOTICS SD MOTOR TYPE: 1CV3312A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 315M, * 132kW (50 Hz) 148kW (60 Hz) 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 5, Flange: FF600 (A660) without motor protection Terminal box at top",12711,"ΤΕΜ",1,"LVM",1,"1LE15033AA235FA4"]
["1LE1503-3AB42-3AA4","SIMOTICS SD MOTOR TYPE: 1CV3314B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 4-pole * Size 315L, * 160kW (50 Hz) 184kW (60 Hz) 3 AC 50Hz 240VD/415VY * 3 AC 60 Hz 480 VY IM B 3, without motor protection Terminal box at top",14286,"ΤΕΜ",1,"LVM",1,"1LE15033AB423AA4"]
["1LE1504-1AA43-1JA4","SIMOTICS SD MOTOR TYPE: 1CV4104A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 60Hz 400VD/690VY IM B 35 * Flange: FF215 (A250) without motor protection Terminal box at top",716,"ΤΕΜ",1,"LVM",1,"1LE15041AA431JA4"]
["1LE1504-1AB41-7JA4","SIMOTICS SD MOTOR TYPE: 1CV4104B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 100L * 2.2kW (50 Hz) 2.55 kW (60 Hz) 3 AC 60 Hz 220 VD/380 VY IM B 35 * Flange: FF215 (A250) without motor protection Terminal box at top",657,"ΤΕΜ",1,"LVM",1,"1LE15041AB417JA4"]
["1LE1504-1AB53-4JA4","SIMOTICS SD MOTOR TYPE: 1CV4105B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF215 (A250) without motor protection Terminal box at top",727,"ΤΕΜ",1,"LVM",1,"1LE15041AB534JA4"]
["1LE1504-1CA02-1JA4","SIMOTICS SD MOTOR TYPE: 1CV4130A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF265 (A300) without motor protection Terminal box at top",1063,"ΤΕΜ",1,"LVM",1,"1LE15041CA021JA4"]
["1LE1504-1CB21-7JA4","SIMOTICS SD MOTOR TYPE: 1CV4132B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 132M, * 7.5kW (50 Hz) 8.6 kW (60 Hz) 3 AC 60 Hz 220 VD/380 VY IM B 35 * Flange: FF265 (A300) without motor protection Terminal box at top",1429,"ΤΕΜ",1,"LVM",1,"1LE15041CB217JA4"]
["1LE1504-1DA32-1JA4","SIMOTICS SD MOTOR TYPE: 1CV4163A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 160M, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2345,"ΤΕΜ",1,"LVM",1,"1LE15041DA321JA4"]
["1LE1504-1DA42-7FA4","SIMOTICS SD MOTOR TYPE: 1CV4164A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 160L, * 18.5 kW (50 Hz) 21.3kW (60 Hz) 3 AC 50 Hz 500 VY 3 AC 60Hz 575VY IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",2730,"ΤΕΜ",1,"LVM",1,"1LE15041DA427FA4"]
["1LE1504-1EA24-0FA4","SIMOTICS SD MOTOR TYPE: 1CV4182A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 180M, * 22kW (50 Hz) 24.5kW (60 Hz) 3 AC 50 Hz 500 VD 3 AC 60 Hz 575 VD IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",3037,"ΤΕΜ",1,"LVM",1,"1LE15041EA240FA4"]
["1LE1504-2AA42-7JA4","SIMOTICS SD MOTOR TYPE: 1CV4204A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 200L, * 30kW (50 Hz) 33.5kW (60 Hz) 3 AC 50 Hz 500 VY 3 AC 60Hz 575VY IM B 35 * Flange: FF350 (A400) without motor protection Terminal box at top",3898,"ΤΕΜ",1,"LVM",1,"1LE15042AA427JA4"]
["1LE1504-2BA24-0JA4","SIMOTICS SD MOTOR TYPE: 1CV4222A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 225M * 45kW (50 Hz) 51kW (60 Hz) 3 AC 50 Hz 500 VD 3 AC 60 Hz 575 VD IM B 35 * Flange: FF400 (A450) without motor protection Terminal box at top",5303,"ΤΕΜ",1,"LVM",1,"1LE15042BA240JA4"]
["1LE1504-2BB21-7AA4","SIMOTICS SD MOTOR TYPE: 1CV4222B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 60 Hz, P60: IE3 4-pole * Size 225M * 45kW (50 Hz) 52kW (60 Hz) 3 AC 60 Hz 220 VD/380 VY IM B 3, without motor protection Terminal box at top",4879,"ΤΕΜ",1,"LVM",1,"1LE15042BB217AA4"]
["1LE1504-2DA20-2FA4","SIMOTICS SD MOTOR TYPE: 1CV4282A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 280M * 90kW (50 Hz) 101kW (60 Hz) 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF500 (A550) without motor protection Terminal box at top",9970,"ΤΕΜ",1,"LVM",1,"1LE15042DA202FA4"]
["1LE1504-2DB22-3AA4","SIMOTICS SD MOTOR TYPE: 1CV4282B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 280M * 90kW (50 Hz) 104kW (60 Hz) 3 AC 50Hz 240VD/415VY * 3 AC 60 Hz 480 VY IM B 3, without motor protection Terminal box at top",9122,"ΤΕΜ",1,"LVM",1,"1LE15042DB223AA4"]
["1LE1504-3AA52-3JA4","SIMOTICS SD MOTOR TYPE: 1CV4315A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 2-pole * Size 315L, * 200kW (50 Hz) 224kW (60 Hz) 3 AC 50Hz 240VD/415VY * 3 AC 60 Hz 480 VY IM B 35 * Flange: FF600 (A660) without motor protection Terminal box at top",21930,"ΤΕΜ",1,"LVM",1,"1LE15043AA523JA4"]
["1LE1504-3AB20-2AA4","SIMOTICS SD MOTOR TYPE: 1CV4312B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line SUPER Premium Efficiency IE4, 4-pole * Size 315M, * 132kW (50 Hz) 152kW (60 Hz) 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B 3, without motor protection Terminal box at top",13104,"ΤΕΜ",1,"LVM",1,"1LE15043AB202AA4"]
["1LE1001-1DB43-4AF4","SIMOTICS GP Motor type: 1AV2164B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 160L, * 15kW (50 Hz) 17.3kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 1 KTY84-130 temperature sensor (2 terminals) Terminal box at top",1601,"ΤΕΜ",1,"LVM",1,"1LE10011DB434AF4"]
["1LE1003-2AB53-4GC6","SIMOTICS GP MOTOR TYPE: 1AV3205B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 200 * 30kW (50 Hz) 34.5kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF350 (A400) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",3303,"ΤΕΜ",1,"LVM",1,"1LE10032AB534GC6"]
["1LE1001-0CA20-2AA4","SIMOTICS GP Motor type: 1AV2072A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 71M * 0.37 kW (50 Hz) 0.43kW(60 Hz) 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B 3, without motor protection Terminal box at top",189,"ΤΕΜ",1,"LVM",1,"1LE10010CA202AA4"]
["1LE1001-0DA22-3JA4","SIMOTICS GP Motor type: 1AV2082A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * Size 80M * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 50 Hz 240 VD/415 VY 3 AC 60 Hz 480 VY IM B 35 * Flange: FF165 (A200) without motor protection Terminal box at top",261,"ΤΕΜ",1,"LVM",1,"1LE10010DA223JA4"]
["1LE1001-0DB33-1JA4","SIMOTICS GP Motor type: 1AV2083B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 80M * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 60Hz 400VD/690VY IM B 35 * Flange: FF165 (A200) without motor protection Terminal box at top",279,"ΤΕΜ",1,"LVM",1,"1LE10010DB331JA4"]
["1LE1001-0EC03-1JA4","SIMOTICS GP Motor type: 1AV2090C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 90S * 0.75kW (50 Hz) 0.86kW (60 Hz) 3 AC 60Hz 400VD/690VY IM B 35 * Flange: FF165 (A200) without motor protection Terminal box at top",325,"ΤΕΜ",1,"LVM",1,"1LE10010EC031JA4"]
["1LE1001-1AC42-3JA4","SIMOTICS GP Motor type: 1AV2104C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * Size 100L * 1.5kW (50 Hz) 1.75 kW (60 Hz) 3 AC 50 Hz 240 VD/415 VY 3 AC 60 Hz 480 VY IM B 35 * Flange: FF215 (A250) without motor protection Terminal box at top",459,"ΤΕΜ",1,"LVM",1,"1LE10011AC423JA4"]
["1LE1001-1CB04-0AA4","SIMOTICS GP Motor type: 1AV2130B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing High Efficiency IE2, In EEA: Minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * Size 132S, * 5.5kW (50 Hz) 6.3kW (60 Hz) 3 AC 50 Hz 500 VD * IM B 3, without motor protection Terminal box at top",706,"ΤΕΜ",1,"LVM",1,"1LE10011CB040AA4"]
["1LE1003-1EB60-4AA4","SIMOTICS GP MOTOR TYPE: 1AV3186B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum enclosure increased power Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 180 * 30kW (50 Hz) 34.5kW (60 Hz) 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box at top",2898,"ΤΕΜ",1,"LVM",1,"1LE10031EB604AA4"]
["1LE1003-2AA53-0AA4","SIMOTICS GP MOTOR TYPE: 1AV3205A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Aluminum housing Premium Efficiency IE3, 2-pole * Size 200 * 37kW (50 Hz) 41.5kW (60 Hz) 3 AC 60 Hz 380 VD/660 VY IM B3 without motor protection Terminal box at top",3742,"ΤΕΜ",1,"LVM",1,"1LE10032AA530AA4"]
["1LE1004-1AA40-2JA4","SIMOTICS GP MOTOR TYPE: 1AV4104A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 100L * 3kW (50 Hz) 3.45kW (60 Hz) 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF215 (A250) without motor protection Terminal box at top",639,"ΤΕΜ",1,"LVM",1,"1LE10041AA402JA4"]
["1LE1004-1BA21-7AA4","SIMOTICS GP MOTOR TYPE: 1AV4112A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 112M, * 4kW (50 Hz) 4.55 kW (60 Hz) 3 AC 60 Hz 220 VD/380 VY IM B 3, without motor protection Terminal box at top",738,"ΤΕΜ",1,"LVM",1,"1LE10041BA217AA4"]
["1LE1004-2AA53-0FA4","SIMOTICS GP MOTOR TYPE: 1AV4205A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) aluminum housing SUPER Premium Efficiency IE4, 2-pole * Size 200L, * 37kW (50 Hz) 41.5kW (60 Hz) 3 AC 60 Hz 380 VD/660 VY IM B 5, flange: FF350 (A400) without motor protection Terminal box at top",4648,"ΤΕΜ",1,"LVM",1,"1LE10042AA530FA4"]
["1LE1004-2AB51-7FA4","SIMOTICS GP Motor type: 1AV4205B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) acc. to 130(B) Aluminum enclosure Super Premium Efficiency IE4, 4-pin * Size 200L* 30 kW (50 Hz) 34.5 kW (60 Hz) 3 AC 60 Hz 220 VD/380 VY IM B 5, flange: FF350 (A400) without motor protection Terminal box at top",3678,"ΤΕΜ",1,"LVM",1,"1LE10042AB517FA4"]
["1LE1501-0CC23-5JA4","SIMOTICS SD MOTOR TYPE: 1CV2072C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line High Efficiency IE2, 6-pole * Size 71M * 0.18kW (50 Hz) 0.21kW (60 Hz) 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 35 * Flange: FF130 (A160) without motor protection Terminal box at top",253,"ΤΕΜ",1,"LVM",1,"1LE15010CC235JA4"]
["1LE1503-1DA62-1JA4","SIMOTICS SD MOTOR TYPE: 1CV3166A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Cast iron frame, increased power Basic line Premium Efficiency IE3, 2-pole * Size 160L, * 22kW (50 Hz) 25.3kW (60 Hz) 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2576,"ΤΕΜ",1,"LVM",1,"1LE15031DA621JA4"]
["1LE1503-1EA20-2JA4","SIMOTICS SD MOTOR TYPE: 1CV3182A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 2-pole * Size 180M, * 22kW (50 Hz) 24.5kW (60 Hz) 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2539,"ΤΕΜ",1,"LVM",1,"1LE15031EA202JA4"]
["1LE1503-1EC43-0JA4","SIMOTICS SD MOTOR TYPE: 1CV3184C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 180L, * 15kW (50 Hz) 18kW (60 Hz) 3 AC 60 Hz 380 VD/660 VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2728,"ΤΕΜ",1,"LVM",1,"1LE15031EC430JA4"]
["1LE1503-2AB62-2JA4","SIMOTICS SD MOTOR TYPE: 1CV3206B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Cast iron frame, increased power Basic line Premium Efficiency IE3, 4-pole * Size 200L, * 37kW (50 Hz) 42.5kW (60 Hz) 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF350 (A400) without motor protection Terminal box at top",3831,"ΤΕΜ",1,"LVM",1,"1LE15032AB622JA4"]
["1LE1503-2BA63-1JA4","SIMOTICS SD MOTOR TYPE: 1CV3226A Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) Cast iron frame, increased power Basic line Premium Efficiency IE3, 2-pole * Size 225M * 55kW (50 Hz) 62kW (60 Hz) 3 AC 60Hz 400VD/690VY IM B 35 * Flange: FF400 (A450) without motor protection Terminal box at top",5571,"ΤΕΜ",1,"LVM",1,"1LE15032BA631JA4"]
["1LE1503-2DB01-8AA4","SIMOTICS SD MOTOR TYPE: 1CV3280B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 280S, * 75kW (50 Hz) 86kW (60 Hz) 3 AC 60 Hz 230 VD/400 VY IM B 3, without motor protection Terminal box at top",6854,"ΤΕΜ",1,"LVM",1,"1LE15032DB018AA4"]
["1LE1503-2DB23-1JA4","SIMOTICS SD MOTOR TYPE: 1CV3282B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * Size 280M * 90kW (50 Hz) 104kW (60 Hz) 3 AC 60Hz 400VD/690VY IM B 35 * Flange: FF500 (A550) without motor protection Terminal box at top",8352,"ΤΕΜ",1,"LVM",1,"1LE15032DB231JA4"]
["1LE1503-3AC22-7AA4","SIMOTICS SD MOTOR TYPE: 1CV3312C Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Basic line Premium Efficiency IE3, 60 Hz, P60: IE2 6-pole * Size 315M, * 90kW (50 Hz) 108kW (60 Hz) 3 AC 50 Hz 500 VY 3 AC 60Hz 575VY IM B 3, without motor protection Terminal box at top",12096,"ΤΕΜ",1,"LVM",1,"1LE15033AC227AA4"]
["1LE1601-3AB03-4GC5","SIMOTICS SD MOTOR TYPE: 1CV2310B Low-voltage motor, IEC Squirrel-cage rotor, self-ventilated, IP55 Temperature class 155(F) according to 130(B) cast iron frame Performance line High Efficiency IE2, In EEA: Minimum efficiency according to applicable statutory regulations ! 4-pole * Size 315S, * 110kW (50 Hz) 127kW (60 Hz) 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, Flange: FF600 (A660) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",10598,"ΤΕΜ",1,"LVM",1,"1LE16013AB034GC5"]
["6AG1132-6BF00-7CA0","SIPLUS ET 200SP -40...+70Β°C start up temperature: -25Β°C with conformal coating based on 6ES7132-6BF00-0CA0 . digital output module, DQ 8x 24VDC/0.5A High Feature suitable for BU type A0, Color code CC02, channel diagnostics",139,"ΤΕΜ",1,"SIMATIC",1,"6AG11326BF007CA0"]
["6AG1138-6BA00-2BA0","SIPLUS ET 200SP TM POSINPUT 1 -40 ... +60Β°C with conformal coating based on 6ES7138-6BA00-0BA0. Counter and positioning module for RS422 incremental encoder or SSI absolute value encoder, 2 DI, 2DQ",350,"ΤΕΜ",1,"SIMATIC",1,"6AG11386BA002BA0"]
["6AG1222-1HF32-2XB0","SIPLUS S7-1200 SM 1222 8DQ RLY -25...+70Β°C with conformal coating based on 6ES7222-1HF32-0XB0 . Digital output 8 DQ, relay 2 A",222,"ΤΕΜ",1,"S7-1200",1,"6AG12221HF322XB0"]
["6AG1331-7NF00-2AB0","SIPLUS S7-300 SM 331 40-pole -25...+70 Β°C With conformal coating based on 6ES7331-7NF00-0AB0 . Analog input isolated \"8 AI; +/-5/10 V, 1-5 V, +/-20 mA, 0/4 to 20 mA, 16 bit (55 ms), single rooting (50 V com.)",1124,"ΤΕΜ",1,"SIMATIC",1,"6AG13317NF002AB0"]
["6AG1455-2AD00-4AA0","SIPLUS D455-2 DP/PN 0...+55Β°C with conformal coating based on 6AU1455-2AD00-0AA0 . SIPLUS \"Drive-based \"\"Control Unit\" \"D455-2 DP/PN;\"\" \"\"Programmable\" \"motion controller \"\"ULTRA-High\" \"Performance;\"\" Interfaces: 12\" DI, 16 DI/DO, 6 DRIVE-CLiQ, 2 PROFIBUS, 3 PROFINET ports, 2 \"Ethernet, 2 USB, \"\"1 option\" \"slot;\"\" incl. dual fan/ battery\" module and battery",10175,"ΤΕΜ",1,"SIMATIC",1,"6AG14552AD004AA0"]
["6AG1512-1DK01-2AB0","SIPLUS ET 200SP CPU 1512SP-1 PN -40...+60Β°C with conformal coating based on 6ES7512-1DK01-0AB0 . CPU 1512SP-1 PN for ET 200SP, Central processing unit with Work memory 200 KB for program and 1 MB for data, first interface: PROFINET IRT with 3-port switch, 48 ns bit performance, SIMATIC Memory Card required, BusAdapter required for port 1 and 2",1512,"ΤΕΜ",1,"SIMATIC",1,"6AG15121DK012AB0"]
["6AG2132-6BH01-4BA0","SIPLUS ET 200SP DQ 16X24VDC/ 0.5A TX RAIL -40Β…+70Β°C TX with 85Β°C for 10min with conformal coating based on 6ES7132-6BH01-0BA0 . (PNP,P-switching) Packing unit: 1 piece, fits to BU-type A0, Colour Code CC00, substitute value output, module diagnostics for: short-circuit to L+ and ground, wire break, supply voltage",203,"ΤΕΜ",1,"SIMATIC",1,"6AG21326BH014BA0"]
["6AG2241-1AH32-1XB0","SIPLUS S7-1200 CM1241 RS232 T1 RAIL -25... +55Β°C T1 with 70Β°C for 10 min with conformal coating based on 6ES7241-1AH32-0XB0 . Communication module RS232, 9-pole D-sub (socket), supports Freeport",333,"ΤΕΜ",1,"S7-1200",1,"6AG22411AH321XB0"]
["6AG4025-0DB10-0BB0","SIMATIC IPC527G (Box PC); 2x Gigabit Ethernet (IE/PN); 1x display port, 1x VGA; 4x USB3.0; 2x RS232/485/422 (can be selected); 100/240 V AC power supply Core i7-6700 (4C/4T, 3.4 (4.0) GHz, 8 MB cache) 1 TB HDD 4 GB DDR4 Without operating system; 1 x PCIe x16 1 x PCIe x1; 2 x PCI 2 x RS232; 2 x USB2.0 additionally",2404,"ΤΕΜ",1,"SIMATIC",1,"6AG40250DB100BB0"]
["6AG4104-4JR42-0XX2","SIMATIC IPC547G (Rack PC, 19\", 4HU); Interfaces: 2x USB 3.0 on the front; 2x Intel Gigabit Ethernet, 2x PS/2, Audio on the rear side; 7 slots: 5x PCI Express, 2x PCI, Temperature and Fan monitoring; Watchdog; Card retainer Xeon E3-1275 v5 (4C/8T, 3.6 (4.0) GHz, 8 MB cache, iAMT); Mainboard: (chipset C236, 1x DVI-D, 2x display ports V1.2, 4x USB 3.0 and 4x USB 2.0 on the rear side, 1x USB 2.0 internal, 1x COM 1; RAID onboard) RAID1, 2 TB (2x 2 TB HDD Enterprise), in interchangeable insert hot-swap and 1x 2 TB HDD Enterprise as hot spare in interchangeable insert, front-side 64 GB DDR4 SD-RAM (4x 16 GB), Dual Channel Enclosure blue chromated, 100/240V AC industrial power supply unit, DVD +/-RW (slim) Graphics onboard Without operating system without expansions (software) Power supply cable USA",6158,"ΤΕΜ",1,"SIMATIC",1,"6AG41044JR420XX2"]
["6AG4112-2KW86-0GA6","SIMATIC IPC647D (Rack PC, 19\", 2 HU); 2x Gbit Ethernet (IE/PN), RJ45; 1x DVI-I; 2x display ports; 1x COM 1; 2x PS/2; audio; 4x USB 3.0, incl. 1x internal; 3x USB 2.0; Temp. and fan monitoring; Watchdog, Card retainer XEON E3-1268LV3 (4C/8T, 2.3 (3.3) GHz, 8 MB cache VT-D, AMT); mainboard without fieldbus RAID1, 240 GB (2x 240 GB SSD SATA mirror disks), in removable frame, hot swap; front-side 32 GB DDR3 SD-RAM (4x 8 GB), ECC, Dual channel Bus module 2 slots: 2x PCIE X16; 1x 240 GB SSD (for operating system), internal without expansion (HW); Graphics onboard Windows Server 2012 R2 Standard Edition incl. 5 clients, 64 bit, MUI (de, en, fr, es, it) SIMATIC PC DiagMonitor V5.0 enclosed 2x 110/240V redund. power supply; without line cable",7940,"ΤΕΜ",1,"SIMATIC",1,"6AG41122KW860GA6"]
["6AG4114-2DB33-0BC0","SIMATIC IPC847D (Rack PC) (Rack PC, 19\", 4HU); 2x Gbit Ethernet (IE/PN), RJ45; 1x DVI-I; 2x display ports; 1x COM 1; 2x PS/2; audio; 4x USB 3.0 incl. 1x internal; 3x USB 2.0; Temp. and fan monitoring; Watchdog, Card retainer Core I3-4330TE (2C/4T, 2.4 GHz, 4 MB cache); mainboard without fieldbus 500 GB HDD SATA, internal 0.5 G vibration, 5 G shock 8 GB DDR3 SD-RAM (2x 4 GB), Dual channel Bus module 11 slots: 3x PCI, 3x PCIE X4, 5x PCIE X16; DVD +/-RW (SLIM) without expansion (HW); Graphics onboard Windows 7 Ultimate, 64 bit, MUI (de, en, fr, es, it), SP1 SIMATIC PC DiagMonitor V5.0 and Image&Partition Creator V3.5 enclosed 110/240V industrial power supply unit; with NAMUR, Power supply cable Europe",3257,"ΤΕΜ",1,"SIMATIC",1,"6AG41142DB330BC0"]
["6AG4114-3DQ02-0AX0","SIMATIC IPC847E (Rack PC, 19\", 4HU); 3x Gbit Ethernet (IE/PN), RJ45; 1x DVI-D; 2x display ports; 1x COM 1; audio, 4x USB 3.1, 2x USB 3.1 (Type C) on the rear side; 2x USB 3.0 on the front; 1x USB 3.1 internal, temperature and fan monitoring; Watchdog, card retainer Core i5-8500 (6C/6T, 3.0 (4.1) GHz, 9 MB cache, TB, VT-d, AMT); Board 9 slots: 7x PCI, 2x PCIe x16 (8 L); 480 GB SSD 2.5\" SATA; Enclosure with drive support Type B (for internal installation/ 0.5 g vibration, 5 g shock); 100/240 V AC industrial power supply unit; 16 GB DDR4 SDRAM (2x 8 GB), Dual Channel; Without extension (HW); Windows10 Enterprise 2016 LTSB, MUI (de, en, fr, it, es), 64-bit (for Core i3/i5); Without expansions; Without power supply cable",3518,"ΤΕΜ",1,"SIMATIC",1,"6AG41143DQ020AX0"]
["6AG4131-2DN31-1BB0","SIMATIC IPC627D (Box PC), HD graphic onboard, 2x Gigabit Ethernet (IE/PN) 4xUSB V3.0; 1x serial (COM 1); RAID controller onboard; Watchdog, temp./fan monitoring Core I3-4330TE (2C/4T, 2.4 GHz, 4 MB cache, VT-X) Solid-state drive 240 GB; 320 GB HDD SATA (2.5\") 8 GB DDR3 1600 DIMM; 1x PCIE (X16); 1x PCI 2x USB additive (1 slot occupied) Windows 7 Ultimate 64 bit SP1, MUI (de, en, fr, es, it) SIMATIC IPC Image&Partition Creator enclosed AC 110/230V industrial power supply unit with NAMUR; Power supply cable Europe",3448,"ΤΕΜ",1,"SIMATIC",1,"6AG41312DN311BB0"]
["6AG4131-2JN60-1XX6","SIMATIC IPC627D (Box PC), HD graphic onboard, 2x Gigabit Ethernet (IE/PN) 4xUSB V3.0; 1x serial (COM 1); RAID controller onboard; Watchdog, temp./fan monitoring XEON E3-1268LV3 (4C/8T, 2.3 (3.3) GHz, 8 MB cache VT-D, AMT); PROFINET (IRT, 3 ports, CP 1616-compatible); 2 MB buffered SRAM Solid-state drive 240 GB; 320 GB HDD SATA (2.5\") 16 GB DDR3 1600 DIMM; ECC; 2x PCI 2x USB additive (1 slot occupied) without operating system without expansion (software) 24 V DC industrial Power supply",4655,"ΤΕΜ",1,"SIMATIC",1,"6AG41312JN601XX6"]
["6AG4132-2DE20-0AX3","SIMATIC IPC827D (Box PC) HD graphic onboard, 2x Gigabit Ethernet (IE/PN) 4xUSB V3.0; 1x serial (COM 1); RAID controller onboard; Watchdog, temp./fan monitoring Core I3-4330TE (2C/4T, 2.4 GHz, 4 MB cache, VT-X) 1 TB HDD SATA; DVD +/-RW 4 GB DDR3 1600 DIMM; 1x PCIE (X16); 1x PCIE (X4); 3x PCI without expansion (HW) Windows 7 Ultimate 32 bit SP1, MUI (de, en, fr, es, it) without expansion (software) AC 110/230V industrial power supply unit with NAMUR; Power supply cable USA",3194,"ΤΕΜ",1,"SIMATIC",1,"6AG41322DE200AX3"]
["6AG4141-5CB34-0FA0","SIMATIC IPC427E (Microbox PC), HD graphic onboard, 4x USB V3.0 (high current), PCIE (optional), Core i5-6442EQ; 3x Gbit Ethernet (IE/PN); Wall mounting; 8 GB; 2x RS232/485; without PCIe; Windows 7 Ultimate SP1, 64-bit, MUI (de, en, es, fr, it); Without replaceable mass storage; 240 GB solid-state drive SATA Without SIMATIC software; 24 V DC industrial power supply",2832,"ΤΕΜ",1,"SIMATIC",1,"6AG41415CB340FA0"]
["6AG4141-7BC04-5GA0","SIMATIC IPC427E (Microbox PC), HD graphic onboard, 4x USB V3.0 (high current), PCIE (optional), XEON E3-1505L; 3x Gbit Ethernet (IE/PN); Mounting onto standard rail; 16 GB; Without RS232/485, without PCIe; Windows 7 Ultimate SP1, 64-bit, MUI (de, en, es, fr, it); CFast 128 GB, (only as option with operating system/SW, if no internal mass storage); 480 GB solid-state drive SATA Without SIMATIC software; 24 V DC industrial power supply",4339,"ΤΕΜ",1,"SIMATIC",1,"6AG41417BC045GA0"]
["6AV2101-4BB06-0AE5","SIMATIC WinCC Comfort V16 upgrade WinCC flexible 2008 Standard-> WinCC Comfort V16 Combo; Engineering software in the TIA Portal; Floating License; SW and documentation on DVD; License key on a USB flash drive; Class A; 6 languages: de,en,fr,es,it,zh; for configuration of SIMATIC Panels. Please observe product release: support.industry.siemens.com Entry ID: 109771219 ******************************* Content: set (3x DVD + 1x USB)",331,"ΤΕΜ",1,"SIMATIC",1,"6AV21014BB060AE5"]
["6AV2103-0HA00-0AQ0","EPL Royalty for SIMATIC WinCC Professional 4096 Power Tags, only valid in connection with Enterprise License contract, requires EPL Master",2896,"ΤΕΜ",1,"SIMATIC",1,"6AV21030HA000AQ0"]
["6AV2104-0HA06-0AH0","SIMATIC WinCC Runtime Advanced 4096 Power Tags V16, Runtime software in TIA Portal; Single License; software, documentation and License key for download; Class A; 6 languages: de,en,fr,es,it,zh; Please observe product release: support.industry.siemens.com Entry ID: 109771219 ******************************* e-mail address mandatory for delivery",3150,"ΤΕΜ",1,"SIMATIC",1,"6AV21040HA060AH0"]
["6AV2105-0XA00-0AL0","SIMATIC WinCC RT Professional Software Update Service (SUS); Within the framework of this contract, you will receive updated software versions for a period of one year, if it is not cancelled three months prior to its expiration. Period of delivery and performance: 1 year from date of invoice. Prerequisite for contract: Current version of the software",1294,"ΤΕΜ",1,"SIMATIC",1,"6AV21050XA000AL0"]
["6AV2105-2FH05-0BJ0","SIMATIC WinCC RT Professional, PowerPack 2048 PowerTags -> 4096 PowerTags V15 (without version change), runtime software in TIA Portal, Single license, without SW, without documentation, License key download, Class A, ******************************* E-mail address required for delivery",469,"ΤΕΜ",1,"SIMATIC",1,"6AV21052FH050BJ0"]
["6AV2108-0DF00-0BH0","SIMATIC Energy Suite S7-1500, Single Runtime License Download contains license certificate for 10 energy objects (2x5 EnO) as pdf for download, Class A; executable on all S7-1500 CPU (without S7-1500S) and ET 200SP CPU Firmware V2.0 or higher ******************************* E-mail address required for delivery",420,"ΤΕΜ",1,"SIMATIC",1,"6AV21080DF000BH0"]
["6AV2124-0UC02-0AX1","SIMATIC HMI TP1900 Comfort, Comfort Panel, Touch operation, 19\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 24 MB configuration memory, WEC 2013, configurable from WinCC Comfort V14 SP1 with HSP",3921,"ΤΕΜ",1,"SIMATIC",1,"6AV21240UC020AX1"]
["6AV2143-8MB50-0AA0","SIMATIC HMI, IWP1200, Industrial Web panel, key/touch operation, 12\" TFT display, 65536 colors, PROFINET interface, HTML5, stand-alone, no WinCC configuration required, contains Open Source software, which is provided free of charge",1607,"ΤΕΜ",1,"SIMATIC",1,"6AV21438MB500AA0"]
["6AV2154-0XB00-0LR0","EPL Maintenance for SIMATIC WinCC Unified PC Runtime max. PowerTags; only valid in connection with Enterprise License agreement, requires EPL Master ******************************* E-mail address required for delivery",3360,"ΤΕΜ",1,"SIMATIC",1,"6AV21540XB000LR0"]
["6AV2156-1CL00-0LB0","SIMATIC WinCC Unified Line Coordination; Extension +5 units; Option for WinCC Unified, runtime software, Single License, license key for download, ******************************* E-mail address required for delivery",1575,"ΤΕΜ",1,"SIMATIC",1,"6AV21561CL000LB0"]
["6AV2185-8EF01-0AA0","Extension unit 19\" KP12F PN for mounting on all fully IP65-protected 16:9 HMI/IPC devices. For the flexible installation of operator controls, 6 mounting positions, 6 operator controls equippable. Connection via PROFIsafe (without equipment)",1028,"ΤΕΜ",1,"SIMATIC",1,"6AV21858EF010AA0"]
["6AV6362-4AH00-0AH0","WinCC/Industrial-Data-Bridge, 3000 tags (countable), Option for WinCC V7.4 or higher, and WinCC Prof. V14 or higher, Data exchange with databases and OPC servers, runtime software, Single license, License key download ******************************* E-mail address required for delivery",3150,"ΤΕΜ",1,"SIMATIC",1,"6AV63624AH000AH0"]
["6AV6371-1KV17-4BX3","WinCC/Audit RC Upgrade from V7.X to V7.4 for WinCC/Audit RC, and WinCC/Change-Control, Runtime/Configuration software, Single license, SW and License Key Download ******************************* E-mail address required for delivery",844,"ΤΕΜ",1,"SIMATIC",1,"6AV63711KV174BX3"]
["6AV6372-2CG20-0EA0","WinCC/Performance Mon. Arch., 1000 archive variables, for WinCC V7.2 or higher, runtime software, single license, count relevant, License key on USB flash drive ******************************* Content: 1x USB",30129,"ΤΕΜ",1,"SIMATIC",1,"6AV63722CG200EA0"]
["6AV6372-2DF67-1BH0","SIMATIC Energy Manager PRO Consumer Package 5; including EE-Monitor; increases the number of consumers by 5 consumers; Engineering/Runtime software; Single license License key for download; without software and documentation ******************************* E-mail address required for delivery",2100,"ΤΕΜ",1,"SIMATIC",1,"6AV63722DF671BH0"]
["6AV6381-2BP07-0AQ0","EPL Royalty for WinCC V7, RC2048 (2048 PowerTags) only valid in connection with Enterprise License agreement, requires EPL Master",7817,"ΤΕΜ",1,"SIMATIC",1,"6AV63812BP070AQ0"]
["6AV6381-2BU07-5AX0","WinCC system software V7.5 SP1, RC 153600 (153600 PowerTags), runtime/configuration software on DVD, Floating License, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), Please observe product release: support.industry.siemens.com SIOS entry ID: 109772767 ******************************* Content: Set (3x DVD + 1x USB)",14543,"ΤΕΜ",1,"SIMATIC",1,"6AV63812BU075AX0"]
["6AV6612-0AA00-0AM0","SIMATIC WinCC Comfort Software Update Service Compact for multiple orders on one position, these deliveries are grouped. Minimum order quantity: 3 units within the framework of this contract, you will receive for one year all up-to-date software versions. the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: current version of the software",155,"ΤΕΜ",1,"SIMATIC",1,"6AV66120AA000AM0"]
["6AV6618-7HB01-3AB0","SIMATIC WinCC flexible /Audit for SIMATIC Panel, runtime software, single license, license key on USB flash drive, for use with SIMATIC Panel series 270/370 ******************************* Content: 1x USB",810,"ΤΕΜ",1,"SIMATIC",1,"6AV66187HB013AB0"]
["6AV6881-0AW11-3AA0","Transport bag for basic tablet with shoulder strap, can be positioned freely, Multifunctional modular design expandable Further information, Quantity and content: see technical data",94.5,"ΤΕΜ",1,"SIMATIC",1,"6AV68810AW113AA0"]
["6AV7241-1BA31-3AA0","SIMATIC IPC 477E 15\" touch (1280 x 800); with front USB; 4 USB (back), Ethernet (10/100/1000); Celeron G3902E; 3x Gbit Ethernet (IE/PN); 4 GB 2x RS 232/RS 485; without PCIe; Win Embedded Standard 7 SP1, English, 32-bit, CFAST 8 GB, (only optionally with operating system/SW, if no internal mass storage); without internal mass storage; Without SIMATIC software; 24 V DC industrial power supply",2763,"ΤΕΜ",1,"SIMATIC",1,"6AV72411BA313AA0"]
["6AV7241-5LB07-0JA0","SIMATIC IPC 477E 22\" Multitouch (1920 x 1080); 4 USB (back), Ethernet (10/100/1000); Core i5-6442EQ; 3x Gbit Ethernet (IE/PN); 8 GB; without RS 232/RS485; without PCIe; Windows 10 IoT Enterprise 2016 LTSB (64-bit) for Celeron, i3 and i5; Without replaceable mass storage; 320 GB HDD SATA; Without SIMATIC software; 24 V DC industrial power supply",4186,"ΤΕΜ",1,"SIMATIC",1,"6AV72415LB070JA0"]
["6AV7260-0AA10-0AX6","SIMATIC IPC677D (Panel PC), 2x10/100/1000 Mbit/s Ethernet; 4x USB V3.0, 1x serial (COM1); Watchdog, temperature and Fan monitoring; RAID controller onboard; 15\" Touch (1280x 800); with front USB Celeron G1820TE (2C/2T, 2.2 GHz, 2 MB cache) 500 GB HDD SATA; 2 GB DDR3 1600 DIMM; 2x PCI without expansion (HW) Windows 7 Ultimate 32 bit SP1, MUI (de, en, fr, es, it) without expansion (software) 24 V DC industrial Power supply",3788,"ΤΕΜ",1,"SIMATIC",1,"6AV72600AA100AX6"]
["6AV7260-1DB10-3EX3","SIMATIC IPC677D (Panel PC), 2x10/100/1000 Mbit/s Ethernet; 4x USB V3.0, 1x serial (COM1); Watchdog, temperature and Fan monitoring; RAID controller onboard; 19\" Touch (1366x 768); with front USB Core I3-4330TE (2C/4T, 2.4 GHz, 4 MB cache, VT-X) 500 GB HDD SATA; DVD +/-RW; 2 GB DDR3 1600 DIMM; 2x PCI 2x USB additive; COM2; LPT (2 slots occupied) Windows 10 Enterprise LTSB 2016, 64 bit, MUI (en, de, fr, it, es) for Celeron and I3; without expansion (software) AC 110/230V industrial power supply unit with NAMUR; Power supply cable USA",4460,"ΤΕΜ",1,"SIMATIC",1,"6AV72601DB103EX3"]
["6AV7261-0DJ40-0AC0","SIMATIC IPC677E(Panel PC), 19\" Multitouch (1920x1080); UHD graphic onboard; DP/DVI-D; 3x Gigabit Ethernet (IE/PN); 6x USB 3.1 Gen. 2; 1x serial (COM 1); RAID controller onboard; Watchdog, temperature and fan monitoring; Core i3-8100 (4C/4T, 3.6 GHz, 6 MB cache, VT-d); NVRAM; M.2 SSD NVMe 512 GB; 64 GB DDR4-2666(4x16); 24 V DC industrial power supply Windows 10 Enterprise 2016 LTSB, 64 bit, MUI (en, de, fr, it, es) For Celeron and Core i3; Without extension (software); Device without CMOS battery (CR2450N); 2x PCI",5968,"ΤΕΜ",1,"SIMATIC",1,"6AV72610DJ400AC0"]
["6AV7674-1MG00-0AA0","illuminated pushbutton for extension units, 22mm, round, plastic, momentary contact, with integrated white LED, with 5 colored lens (colorless, yellow, red, green, blue),1 NO and 1 NC, w/o inscription (incl. PCB and contact module)",30.1,"ΤΕΜ",1,"SIMATIC",1,"6AV76741MG000AA0"]
["6AV7860-0CH50-0AA0","SIMATIC Flat Panel Connecting cable Industrial Grade USB 5 m",21,"ΤΕΜ",1,"SIMATIC",1,"6AV78600CH500AA0"]
["6AV7863-4AA00-0AA0","SIMATIC IFP2200 Flat Panel 22\" display (16: 9), without touch, only display, Standard up to 5 m, 1920x 1080 pixels, for 24 V DC, display port/DVI interface incl. DVI cable 1.8 m",1470,"ΤΕΜ",1,"SIMATIC",1,"6AV78634AA000AA0"]
["6AV7882-0AA10-3MA0","SIMATIC IPC277E (Nanopanel PC); 7\" Touch TFT; 2x 10/100/1000 Mbps Ethernet RJ45; 1x display port graphic; 1x USB 3.0; 2x USB 2.0; 1x serial (COM 1); CFast slot; 24 V DC power supply Celeron N2807 (2C/2T) 2 GB RAM; WIN Embedded Standard 7 P SP1, English; 32 bit 16 GB CFAST; without SIMATIC software",1957,"ΤΕΜ",1,"SIMATIC",1,"6AV78820AA103MA0"]
["6AV7882-0HB30-7CA0","SIMATIC IPC277E (NANOPANEL PC); 12\" MULTITOUCH (1280 X 800); 2 X 10/100/1000 MBIT/S ETHERNET RJ45; 1X DISPLAY-PORT GRAPHIC; 1 X USB 3.0; 3 X USB 2.0; 1 X SERIAL (COM1); CFAST-SLOT; 24V DC POWER SUPPLY; Celeron N2930 (4C/4T) 8 GB RAM; Windows 10 IoT Enterprise LTSB 2016, 64 bit, MUI (en,de,fr,it,es) 240 GB SSD without SIMATIC software",2660,"ΤΕΜ",1,"SIMATIC",1,"6AV78820HB307CA0"]
["6BK1900-6BA00-0AA0","replacement part SIPLUS HCS4000 connector set for PM DI/DQ consisting of 8 plugs",92,"PAK",1,"SIMATIC",1,"6BK19006BA000AA0"]
["6EP1331-1LD00","PSU100D 24 V/2.1 A Stabilized power supply input: 100-240 V AC output: DC 24 V/2,1 A",45.2,"ΤΕΜ",1,"SIMATIC",1,"6EP13311LD00"]
["6EP1935-6ME21","SITOP Akkumodul 24 V/7 Ah with maintenance free Seaed lead batteries for SITOP DC-USV Module 6 A, 15 A and 40 A",132,"ΤΕΜ",1,"SIMATIC",1,"6EP19356ME21"]
["6EP4136-3AB00-2AY0","SITOP UPS1600 20 A Ethernet/ PROFINET Uninterrupted power supply with Ethernet / PROFINET interface / OPC UA Server / Web server input: 24 V DC output: 24 V DC/20 A",324,"ΤΕΜ",1,"SIMATIC",1,"6EP41363AB002AY0"]
["6ES7131-4FB00-0AB0","SIMATIC DP, 5 electronic modules for ET 200S, 2 DI 230 V AC 15 mm width, 5 units per packing unit",251,"PAK",1,"SIMATIC",1,"6ES71314FB000AB0"]
["6ES7141-6BF00-0AB0","SIMATIC DP, ET 200ECO PN, 8 DI 24 V DC; 4xM12, Duplicate assignment, Degree of protection IP67",251,"ΤΕΜ",1,"SIMATIC",1,"6ES71416BF000AB0"]
["6ES7142-6BR00-0AB0","SIMATIC DP, ET 200ECO PN, 8 DO 24 V DC/2 A; 8xM12, Degree of protection IP67",454,"ΤΕΜ",1,"SIMATIC",1,"6ES71426BR000AB0"]
["6ES7193-4CE10-0AA0","SIMATIC DP, Terminal module TM-P15C22-01 for ET 200S for power modules, 15 mm width, spring-type terminals (Cage Clamp) 2x2 terminal connections without terminal access to AUX1, AUX1 continuous",10,"ΤΕΜ",1,"SIMATIC",1,"6ES71934CE100AA0"]
["6ES7194-2LH02-0AD0","Connecting cable for Bus cable for ET connection M8 assembled on both ends with 2x M8 socket, 4-pole, shielded Length 0,2m",20.400000000000002,"ΤΕΜ",1,"SIMATIC",1,"6ES71942LH020AD0"]
["6ES7194-2MN15-0AB0","bus cable for ET connection M8, PUR cable assembled on both ends with 2x M8 connectors angled, 4-pole, shielded Length 15 m",86.8,"ΤΕΜ",1,"SIMATIC",1,"6ES71942MN150AB0"]
["6ES7195-7HF80-0XA0","SIMATIC DP, bus module BM DP/PA for extended temperature range Bus module for DP/PA coupler for insertion and removal function during operation",69.3,"ΤΕΜ",1,"SIMATIC",1,"6ES71957HF800XA0"]
["6ES7292-1AL40-0XA0","SIMATIC S7-1200, spare part, I/O terminal block tin-coated, coded right, Digital signal module 32CH (4 units with 11 screws each)",39.1,"PAK",1,"S7-1200",1,"6ES72921AL400XA0"]
["6ES7323-1BH01-0AA0","SIMATIC S7-300, Digital module SM 323, isolated, 8DI and 8DO, 24 V DC, 0.5 A Total current 2A, 1x 20-pole",305,"ΤΕΜ",1,"SIMATIC",1,"6ES73231BH010AA0"]
["6ES7326-2BF41-0AB0","SIMATIC S7, Digital output SM 326, F-DO 8x24 V DC/2A PM fail-safe digital output Switching to P-M potential up to Category 4 (EN 954-1)/ SIL3 (IEC61508)/PLE (ISO13849), 1x 40-pole",1047,"ΤΕΜ",1,"SIMATIC",1,"6ES73262BF410AB0"]
["6ES7392-2XX00-0AA0","SIMATIC S7-300, Labeling strips (spare part),for size with 20-pole front connector, 10 units per packing unit",8.2999999999999989,"PAK",1,"SIMATIC",1,"6ES73922XX000AA0"]
["6ES7592-1BM00-0XA0","SIMATIC S7-1500, Front connector in push-in design, 40-pole for 25 mm wide modules and compact CPUs of the S7-1500, incl. cable tie",36.200000000000003,"ΤΕΜ",1,"SIMATIC",1,"6ES75921BM000XA0"]
["6ES7647-8BA32-6EA1","SIMATIC IPC227E (Nanobox PC); 1x display port; 2x 10/100/1000 Mbit/s Ethernet RJ45; 1 x USB3.0, 3 x USB2.0; CFast slot; 24 V DC industrial power supply Celeron N2807 (2C/2T) 8 GB RAM; Box: Basis with COM 1/2 Windows 7 Ultimate SP1, 64 bit; MUI (de, en, fr, es, it) 128 GB SSD; without SIMATIC software DIN rail mounting",1697,"ΤΕΜ",1,"SIMATIC",1,"6ES76478BA326EA1"]
["6ES7648-1AA01-0XE0","Tower kit, for conversion of the rack PC to industrial tower PC, for SIMATIC IPC547G (Device with short housing)",57.800000000000004,"ΤΕΜ",1,"SIMATIC",1,"6ES76481AA010XE0"]
["6ES7648-6GA84-0YX0","SIMATIC IPC FirmwareManager V4.0 (for 50 devices); Software for configuration and updating of firmware components; For mobile use with up to 50 SIMATIC IPCs; single license; Software and License for download ******************************* E-mail address required for delivery .",314,"ΤΕΜ",1,"SIMATIC",1,"6ES76486GA840YX0"]
["6ES7718-1DB04-1AB1","SIMATIC Field PG M6 Advanced; i7-8850H (2.6 to 4.3 GHz; 6 kernels + hyper-threading; 9 MB Smart Cache); 15.6\" display; Full HD (1920x 1080); WLAN 802.11ac & Bluetooth V5.0; DVD +/-RW; UHD Graphics 630; 2x 32 GB DDR4 SD-RAM SO-DIMM; 512 GB SSD SATA (2.5\"); without S5 interface, without S5-EPROMMER Line cable with power plug: USA; Keyboard: QWERTZ/QWERTY; 512 GB SSD  NVME (M.2); Windows 10 Enterprise (Version 1903), 64-bit; License for STEP 7 Professional V16; WinCC Advanced V16; Safety Advanced V16; SINEMA RC Client 2.0; Version of software V16.0.0.0",9051,"ΤΕΜ",1,"SIMATIC",1,"6ES77181DB041AB1"]
["6ES7810-4CC11-0YA6","SIMATIC S7, STEP 7 V5.6 SP2, data carrier incl. Rental License for 50 hours, E-SW, SW and docu. on DVD, license key on USB flash drive, Class A, 5 languages (de,en,fr,es,it), executable in Windows Server 2008 R2 SP2, Windows Server 2012 R2, Windows Server 2016, Windows Server 2019, Windows 7 SP2, Windows 10 Professional, Windows 10 Enterprise Reference HW: S7-300/400, C7 ******************************* Content: Set (1x DVD + 1x USB)",424,"ΤΕΜ",1,"SIMATIC",1,"6ES78104CC110YA6"]
["6ES7823-1EA00-0YL5","TIA Portal Teamcenter Gateway Software Update Service (SUS) for TIA Portal Teamcenter gateway Within the framework of this contract, you will receive for one year all up-to-date software versions. The contract is extended automatically by 1 year if it is not canceled 3 months prior to before expiration. Period of delivery and performance 1 year from date of invoice Requirement for conclusion: Current version of the software",236,"ΤΕΜ",1,"SIMATIC",1,"6ES78231EA000YL5"]
["6ES7833-1FC00-0YL0","STEP 7 Safety Advanced F-programming tool SUS for UCL Unlock Copy License, Software Update Service within the framework of this contract, you will receive for one year all up-to-date software versions. the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice Requirement for conclusion: Unlock Copy License agreement",92.4,"ΤΕΜ",1,"SIMATIC",1,"6ES78331FC000YL0"]
["6ES7921-3AA00-0AA0","Front connector module with flat ribbon Cable connection for digital 16 I/O modules of the S7-300, Power supply over Spring terminals",46.2,"ΤΕΜ",1,"SIMATIC",1,"6ES79213AA000AA0"]
["6ES7921-5AJ00-0AA0","Front connector module with 1x16 pole IDC connector for digital 2 A output modules of the S7-1500 Potential supply over Push-in terminal",53.6,"ΤΕΜ",1,"SIMATIC",1,"6ES79215AJ000AA0"]
["6ES7923-0BC00-0CB0","Connecting cable unshielded for SIMATIC S7-300/1500 between front connector module and Connection module 16x0.14 mm2 with IDC connectors, Length = 2.0 m",21,"ΤΕΜ",1,"SIMATIC",1,"6ES79230BC000CB0"]
["6ES7924-2AK20-0BA0","Connection module TP1 DI-M read 32 channels a. 4x2 terminals f. Potential supply Type: Screw terminal with LED, VPE = 1 unit 50 pole IDC connector f. cable",55.7,"ΤΕΜ",1,"SIMATIC",1,"6ES79242AK200BA0"]
["6FE1263-8FB10-0AA0","SIMATIC ECC CHAdeMO, function block single license, e-vehicle communication acc. to CHAdeMO 1.x-2.0 specification. In connection with SIMATIC PN/CA 6BK1620-0AA00-0AA0 or ET 200SP CM CAN 6ES7137-6EA00-0BA0",210,"ΤΕΜ",1,"SIMATIC",1,"6FE12638FB100AA0"]
["6GK1704-1VW03-0AA0","Industrial Ethernet SOFTNET Security Client V3.0 software for setting up secure IP based VPN connections from PC/PG to network segments, by SCALANCE S single license is protected for 1 installation Runtime software, Software and electr. manual on CD-ROM, 5 languages (de, de, fr, en fr, sp, it) ; for 32 bit Windows: 7 Professional, Ultimate XP Professional+SP3",268,"ΤΕΜ",1,"SIMATIC",1,"6GK17041VW030AA0"]
["6GK1901-0DA20-0AA0","MM FO BFOC connector set 20 units for FO cable, Standard, trailing, indoor, ground, FRNC, robust and ship cable Note: for assembly, special tools and specialist personnel are required; gluing and polishing technology",205,"PAK",1,"SIMATIC",1,"6GK19010DA200AA0"]
["6GK5008-0GA10-1AB2","SCALANCE XB008G unmanaged Industrial Ethernet Switch for 10/100/1000 Mbit/s; for setting up small star and line topologies; LED diagnostics, IP20, 24 V DC power supply, with 8x 10/100/1000 Mbit/s RJ45 ports electrical Manual available as a download",541,"ΤΕΜ",1,"SIMATIC",1,"6GK50080GA101AB2"]
["6GK5208-0HA10-2AA6","SCALANCE X208PRO, managed IE switch, 8x 10/100 Mbit/s M12 ports, IP65/67, LED diagnostics, error signaling contact, Redundant power supply, PROFINET IO device, network management, can be operated in redundant ring, dust caps, incl. electronic manual on CD-ROM, C-plug optional",940,"ΤΕΜ",1,"SIMATIC",1,"6GK52080HA102AA6"]
["6GK5308-2GG10-2CA2","SCALANCE X308-2M TS;  managed IE switch, compact; 4x 10/100/1000 Mbit/s for RJ45 ports electrical; 2x 100/1000 Mbit/s for 2-port media modules, electrical or optical; LED diagnostics; error signaling Contact; PROFINET IO device; network management; integrated redundancy manager; Office features (RSTP, VLAN, IGMP,..); C-plug in scope of delivery extended temperature range with railway approval EN 50155;",2583,"ΤΕΜ",1,"SIMATIC",1,"6GK53082GG102CA2"]
["6GK5774-1FX00-0AC0","IWLAN Access Point, SCALANCE W774-1 RJ45, 1 radio, 2 R-SMA antenna port, iFeatures support via key plug, IEEE 802.11a/b/g/h/n, 2.4/5GHz, gross data rate 300 Mbit/s, 2x RJ45 max. 100 Mbit/s, PoE integrated 2-port switch, redundant 24 V DC, terminal block, IP30, -20... 60 Β°C, plug slot WPA2/802.11i/e, observe national approvals! CERT ID: MSN-W1-RJ-E2, scope of delivery: Manuals on CD-ROM, German/English, 1x terminal block; for operation in Israel",882,"ΤΕΜ",1,"SIMATIC",1,"6GK57741FX000AC0"]
["6GK5991-1AB00-8AA0","SCALANCE X accessory STP 991-1; Pluggable for SCALANCE XM-400; 1x 100 Mbit/s ST/BFOC port, optical; multimode optical up to max. 5 km",194,"ΤΕΜ",1,"SIMATIC",1,"6GK59911AB008AA0"]
["6GK5992-2AS00-8FA0","SCALANCE X accessory; Media module MM992-2SFP; with Conformal Coating; 2x 100/1000 Mbit/s for SFP Plug-in transceiver",226,"ΤΕΜ",1,"SIMATIC",1,"6GK59922AS008FA0"]
["6GT2810-2DC10","SIMATIC RF640T Tool Tag; 50x 8 mm (DxH); On-Metal Transponder ISO 18000-6C, EPC Class 1 GEN 2, Frequency 902 to 928 MHz (FCC), Chip type NXP G2XM, EPC 240 bit 64-byte add-on memory, Minimum order quantity 10 units",27.8,"ΤΕΜ",1,"SIMATIC",10,"6GT28102DC10"]
["6XV1440-4BN20","Connecting cable PN for Mobile Panels (PROFINET), special length 20 m",642,"ΤΕΜ",1,"SIMATIC",1,"6XV14404BN20"]
["6XV1821-0BN50","PROFIBUS Plastic Fiber Optic, Standard cable with 4 BFOC connectors, Length 50 m",246,"ΤΕΜ",1,"SIMATIC",1,"6XV18210BN50"]
["6XV1822-5BH50","7/8\" plug-in cable for Power supply of the ET 200, pre-assembled cable with 2 7/8\" connectors, 5-pole, 5 m",63.6,"ΤΕΜ",1,"SIMATIC",1,"6XV18225BH50"]
["6XV1870-3QN15","Industrial Ethernet TP Cord RJ45/RJ45, CAT 6A, TP cable 4x2, pre-assembled with 2 RJ45 connectors, Length 15 m",46.7,"ΤΕΜ",1,"SIMATIC",1,"6XV18703QN15"]
["6XV1873-3AN15","FO Standard Cable 50/125, pre-assembled with 2x2 BFOC connectors, Length 15 m",99.5,"ΤΕΜ",1,"SIMATIC",1,"6XV18733AN15"]
["6XV1873-3DN10","FO Trailing Cable GP 50/125, pre-assembled with 2x2 BFOC connectors, length 10 m",145,"ΤΕΜ",1,"SIMATIC",1,"6XV18733DN10"]
["6XV1878-5BH30","IE connecting cable IE FC RJ45 Plug-180/IE FC RJ45 Plug-180; IE FC flexible GP 4x2 cable Pre-assembled with 2x IE FC RJ45 plug 180 4 x 2; Length 3.0 m",60.9,"ΤΕΜ",1,"SIMATIC",1,"6XV18785BH30"]
["7KG6106-2HN27-0B","Simeas transmitter (G) MUU for alternating voltage in the enclosure, for snapping on standard mounting rail Rated frequency 50 Hz Input voltage 380V AC Output signal DC 4 to 20 mA (live zero) Auxiliary power 45 to 65 Hz AC, 230 V Measuring range linear 0 up to UEN",678,"ΤΕΜ",1,"SIMATIC",1,"7KG61062HN270B"]
["7KG6113-2EN27-0B","Simeas transmitter (G) MUI for alternating current in the enclosure, for snapping on standard mounting rail Rated frequency 50 Hz Input current 5 A Output signal DC 4 to 20 mA (live zero) Auxiliary power 45-65 Hz AC, 230 V Measuring range linear 0 up to IEN",678,"ΤΕΜ",1,"SIMATIC",1,"7KG61132EN270B"]
["7KG6131-1PN24","Simeas T transmitter for direct current, Direct voltage and isolation amplifier Input voltage: 150 V to 150 V DC Output signal: DC 4mA to 20 mA Zero position: Input: 0 mA, V=output: 4 mA Auxiliary power 88 V to 284 V DC",938,"ΤΕΜ",1,"SIMATIC",1,"7KG61311PN24"]
["6ES7400-1TA01-0AA0","SIMATIC S7-400, rack UR1, central and distributed with 18 slots, 2 redundant PS can be plugged in",1060,"ΤΕΜ",1,"SIMATIC",1,"6ES74001TA010AA0"]
["6ES7952-1AM00-0AA0","SIMATIC S7, RAM Memory Card for S7-400, long design, 4 Mbytes",1585,"ΤΕΜ",1,"SIMATIC",1,"6ES79521AM000AA0"]
["6ES7823-1HA02-0YA5","SIMATIC Machine Simulator S V2.0 software incl. SIMIT V10.1 S and PLCsim Advanced V2.0 Floating License for 1 user Engineering software SW and documentation on DVD, Class A, 2 languages (D, E), executable on Win 7 SP1, Win 10 LTSB 2015, Win 10 (1809), Win Server 2012 R2 / 2016, For more information, see SIMIT V10.1 Readme, Reference HW: PG/PC Content: 1x DVD + 1x USB",4988,"ΤΕΜ",1,"SIMATIC",1,"6ES78231HA020YA5"]
["6GK1704-1CW00-3AN0","Industrial Ethernet SOFTNET-S7 V8.0 SW for S7, S5-comp. Comm.; OPC, PG/OP communic., NCM PC, up to 64 connections UCL license package with 20 Single Licenses, R-software Runtime software, Software and electr. manual on CD-ROM, Class A, 2 languages (de, en) for Windows (32 bit) XP pro+SP1, 2 Windows 2000 Pro+SP3, 4, Server Windows 2003 Server for CP 1512/CP 1612/CP 7515 required UCL license agreement",23321,"ΤΕΜ",1,"SIMATIC",1,"6GK17041CW003AN0"]
["6GK1704-5CW00-3AN0","PROFIBUS SOFTNET-S7 V8.0 Software for S7, S5-comp. communication; OPC, PG/OP communication, NCM PC; UCL license package with 20 Single Licenses, Runtime software, Software and electron. manual on CD-ROM, Class A, 2 languages (de, en) for Windows (32 bit) XP pro +SP1, 2, Windows 2000 Pro+SP3, 4, Server; Windows 2003 Server+SP1 for CP 5511/CP 5512/CP 5611/CP 5621 UCL license agreement required",10868,"ΤΕΜ",1,"SIMATIC",1,"6GK17045CW003AN0"]
["6GK1716-0HB13-0AK0","HARDNET-IE S7 REDCONNECT V13 incl. S7 OPC Server, S7-1613 V12 software for fail-safe S7 comm; Single License for 1 installation of runtime software, Software and electr. manual; License key for download; Class A; 2 languages (de, en); for 32/64 bit: Windows 7 SP1 Prof./Ultimate, 64 bit: Windows 8.1 Pro, Windows 10; Server 2008 R2 SP1, 2012 R2 max. 4 CP 1613A2, CP 1623, CP 1628 ******************************* E-mail address required for delivery",2027,"ΤΕΜ",1,"SIMATIC",1,"6GK17160HB130AK0"]
["6GT2780-0DE00","SIMATIC RTLS Locating Manager Replication service, server or client function, option for license Basic, Single License, software and license key download ******************************* E-mail address required for delivery",9030,"ΤΕΜ",1,"SIMATIC",1,"6GT27800DE00"]
["6GT2810-2AC82","SIMATIC RF630L (special version) SmartLabel PET; 45x 20 mm; strongly adhesive on plastic ISO 18000-6C, EPC Class 1 GEN 2 frequency 860 to 960 MHz, Chip type Alien Higgs 4, Memory 128-bit EPC, 128 bit User, Core diameter 76 mm 2500 units on one roll 4 rolls in carton Minimum order quantity 10000 units",32.4,"ΤΕΜ",100,"SIMATIC",10000,"6GT28102AC82"]
["6GT2821-2BC32","SIMATIC RF200 reader RF220R IO-Link interface V1.1; IP67, -25 to +70 Β°C; M30x 83 mm; with integrated antenna 32 Byte IO; 230 Kbps",544,"ΤΕΜ",1,"SIMATIC",1,"6GT28212BC32"]
["6NH9910-0AA31-0AC1","PP TCSB 64 to 256 V3.1; Power Pack for TeleControl Server Basic of 64 to 256 RTUs; to Operation of up to 256 remote stations; License key on USB stick",3665,"ΤΕΜ",1,"SIMATIC",1,"6NH99100AA310AC1"]
["3AX1405-2B","accessory for 3AE1 electrical closing lock-out without measuring element DC 24V",1716,"ΤΕΜ",1,"LP",1,"3AX14052B"]
["3AX1438-6C","accessory for 3AE5 separating shell width across flats 275mm 7.2 up to 12kV up to 25kA up to 1250A shortened",224,"ΤΕΜ",1,"LP",1,"3AX14386C"]
["3AX1453-2B","accessory for 3AE slide-in rails up to 17.5kV up to 40kA",689,"ΣΕΤ",1,"LP",1,"3AX14532B"]
["3AY1410-0J","spare part for 3AE5 operating solenoid as closing solenoid or 1st shunt release AC 100/125V 50/60Hz for 3AE5",394,"ΤΕΜ",1,"LP",1,"3AY14100J"]
["3AY1510-6E","spare part for 3AE operating solenoid AC 100V - 125V 50/60HZ",814,"ΤΕΜ",1,"LP",1,"3AY15106E"]
["3AY1715-6L","spare interrupter assemblies complete for 3AH3425-2/4 3AH3426-2/4 3AH4305-2/4/6",15679,"ΤΕΜ",1,"LP",1,"3AY17156L"]
["3KA5840-1AE01","Switch disconnector in new design Iu=630 A, Ue = 690 V, 4-pole basic version without 8UC6 handle and shaft 4th pole selectable, AC-21A",2155,"ΤΕΜ",1,"LP",1,"3KA58401AE01"]
["3KA7142-3CD00","Change-over switch 3 x 800 A over- lap-WI",8208.4500000000007,"ΤΕΜ",1,"LP",1,"3KA71423CD00"]
["3KA7152-4AE02","Switch disconnector 4 x 1000 A with shunt R",7135.45,"ΤΕΜ",1,"LP",1,"3KA71524AE02"]
["3KA7183-3AA02","Switch disconnector 3x 1250 A W /O HANDLE",3497.98,"ΤΕΜ",1,"LP",1,"3KA71833AA02"]
["3KC4348-0FA21-0AA3","SENTRON, transfer switching equipment 3KC, remotely operated, RTSE, 3-pole, Iu: 800 A, Ue AC: 415 V, Ie at AC-33 B at 415 V: 800 A, Ie at AC-23 A at 690 V: 630 A, screw mounting, motorized operating mechanism, at the right end, long handle, busbar connection",4320,"ΤΕΜ",1,"LP",1,"3KC43480FA210AA3"]
["3KC9000-8TL74","ATC6 expansion module RS485 Accessory for ATC6300 and ATC6500 pluggable contains RS484 interface",228.48,"ΤΕΜ",1,"LP",1,"3KC90008TL74"]
["3KC9804-3","Accessory for 3KC4, 3KC8 Terminal covers 1-pole for 630 A contains 3 units",35.700000000000003,"ΤΕΜ",1,"LP",1,"3KC98043"]
["3KD0433-2LG20-3","Switch disconnector 80A, size 02, 3-pole Front operating mechanism center Complete unit with direct operating mechanism red/yellow Box terminal",83.7,"ΤΕΜ",1,"LP",1,"3KD04332LG203"]
["3KD2840-2ME20-0","SWITCH-DISCONNECTOR 80A, FRAME SIZE 1, 4-POLE FRONT OPERATING CENTER BASIC UNIT WITHOUT HANDLE BOX TERMINAL",90.68,"ΤΕΜ",1,"LP",1,"3KD28402ME200"]
["3KD3430-2NE10-0","Switch disconnector 160 A, Size 2, 3-pole Front operating mechanism left Basic unit without handle Box terminal",133.82999999999998,"ΤΕΜ",1,"LP",1,"3KD34302NE100"]
["3KD4444-0QE40-0","Switch disconnector 500 A, Size 4, 4-pole Side operating mechanism right Basic unit without handle flat terminal",590.34,"ΤΕΜ",1,"LP",1,"3KD44440QE400"]
["3KD9103-5","Accessory for 3KD size 1/2, 3KF size 1 3KC0 size 1/2 Auxiliary switch module for max. 2 auxiliary switches",11.51,"ΤΕΜ",1,"LP",1,"3KD91035"]
["3KD9508-6","Accessory for 3KD size 5 3KF size 5, 3KC0 size 5 Phase barriers contains 6 units",40.28,"ΤΕΜ",1,"LP",1,"3KD95086"]
["3KF3325-0MF51","Switch disconnector with fuse 3KF SITOR, 250 A, Size 3, 3-pole, for LV HRC fuse Sz. 0 and 1 for semiconductor protection, front operating mechanism, central, basic unit without handle, flat terminal without fuses",419.25,"ΤΕΜ",1,"LP",1,"3KF33250MF51"]
["3KF9105-2AA00","Accessory for 3KF size 1 Fourth pole, switchable for LV HRC fuse Sz. 000 box terminal",45.62,"ΤΕΜ",1,"LP",1,"3KF91052AA00"]
["3KL7112-3CA00","Switch disconnector with fuses 3x 45A WI",258.59999999999997,"ΤΕΜ",1,"LP",1,"3KL71123CA00"]
["3KL7121-4DA00","SECTION FUS-NH 4x 100 A SANS COMM",386.28,"ΤΕΜ",1,"LP",1,"3KL71214DA00"]
["3KL7184-3AA51","Switch disconnector with fuses 3 x 1250 A",8068.96,"ΤΕΜ",1,"LP",1,"3KL71843AA51"]
["3KM5330-1GJ01","Switch disconnector with fuse in new design Iu=160 A, Ue = 690 V, 3-pole for BS88 fuse form A4 with isolating contact strip for MCC with door operating mechanism 8UC7 Handle dark blue/blue-green Basic masking frame light gray",1225,"ΤΕΜ",1,"LP",1,"3KM53301GJ01"]
["3KX7112-5EA00","ACCESSORIES for 3KA71 and 3KL71",422.77,"ΤΕΜ",1,"LP",1,"3KX71125EA00"]
["3KX7141-6AA00","CONT AUX 1NO+1NF gR 5",23.17,"ΤΕΜ",1,"LP",1,"3KX71416AA00"]
["3KX7180-4HA00","Access COMM VERR Sz. 4",99.460000000000008,"ΤΕΜ",1,"LP",1,"3KX71804HA00"]
["3LD2164-2TD51-0AE2","SENTRON, Switch disconnector 3LD, main switch, 3-pole, Iu: 25 A, Operating power / at AC-23 A at 400 V: 9.5 kW, molded-plastic encapsulation for metric screw connection, 1 NC, 1 NO, rotary operating mechanism, black",56.94,"ΤΕΜ",1,"LP",1,"3LD21642TD510AE2"]
["3LD2264-2TV51","SENTRON, Switch disconnector 3LD, main switch, 4-pole, Iu: 32 A, Operating power / at AC-23 A at 400 V: 11.5 kW, molded-plastic encapsulation for metric cable gland, rotary operating mechanism, black",63.33,"ΤΕΜ",1,"LP",21,"3LD22642TV51"]
["3LD2548-0TK53-0AB3","SENTRON, Switch disconnector 3LD, emergency switching-off switch, 3- pole, Iu: 63 A, operating power / at AC-23 A 400 V: 22 kW, floor mounting with door coupling, rotary operating mechanism, Red / yellow, central mounting 22.5 mm of the handle, without tolerance compensation",75.989999999999995,"ΤΕΜ",1,"LP",1,"3LD25480TK530AB3"]
["3LD2748-0TK53","SENTRON, Switch disconnector 3LD, emergency switching-off switch, 3- pole, Iu: 100 A, operating power / at AC-23 A 400 V: 37 kW, floor mounting with door coupling, rotary operating mechanism, Red / yellow, central mounting 22.5 mm of the handle, without tolerance compensation",104.49,"ΤΕΜ",1,"LP",1,"3LD27480TK53"]
["3LD3140-1TL13","Load disconnector 3LD3, Iu 25 A Main switch 3-pole + N Rated operating capacity at AC-23 A at 400V 9.0kW floor mounting Basic switch with door coupling Central hole mounting 22.5mm Toggle drive red / yellow 48x48 mm with auxiliary switch 1OE + 1S",44.97,"ΤΕΜ",1,"LP",1,"3LD31401TL13"]
["3LD3330-0TL11","Load disconnector 3LD3, Iu 40 A Main switch 3-pole + N Rated operating capacity at AC-23 A at 400 V 18.5 kW Installation in distribution boards, Basic switch with selector knob black",36.54,"ΤΕΜ",1,"LP",1,"3LD33300TL11"]
["3LD5220-0TK11","SENTRON, Molded case switch 3LD5 UL, Main switch, 3-pole, certified according to UL489 UL60947-4-1 and IEC60947-3, UL: 60A, SCCR 50kA at 480VAC, Operating power at 480VAC 3-phase: 40hp, IEC: 63A, Operating power at AC-23A at 400V: 30kW, front-mounted, rotary operating mechanism, black, 4-hole mounting of the handle, incl. terminal covers for the infeed side",95.58,"ΤΕΜ",1,"LP",1,"3LD52200TK11"]
["3LD9340-3C","PE-through terminal, Floor installation, accessory for Load disconnector 3LD3",7.8,"ΤΕΜ",1,"LP",1,"3LD93403C"]
["3NA3224-6","LV HRC fuse element, NH2, In: 80 A, gG, Un AC: 690 V, Un DC: 440 V, Front indicator, live grip lugs",56.169999999999995,"ΤΕΜ",1,"LP",3,"3NA32246"]
["3NA3830","LV HRC fuse element, NH000, In: 100 A, gG, Un AC: 500 V, Un DC: 250 V, Front indicator, live grip lugs",4.2699999999999996,"ΤΕΜ",1,"LP",3,"3NA3830"]
["3NA6814-4","LV HRC fuse element, NH000, In: 35 A, gG, Un AC: 400 V, Combined indicator, insulated Grip lugs",7.88,"ΤΕΜ",1,"LP",3,"3NA68144"]
["3NA7140","LV HRC fuse element, NH1, In: 200 A, gG, Un AC: 500 V, Un DC: 440 V, Combined indicator, live grip lugs",14.75,"ΤΕΜ",1,"LP",3,"3NA7140"]
["3NC1440-0MK","SITOR cylindrical fuse link, 14x51 mm, 40 A, gR, Un AC: 690 V, Un DC: 440 V",8.77,"ΤΕΜ",1,"LP",10,"3NC14400MK"]
["3NC2220","SITOR cylindrical fuse link, 22x58 mm, 20 A, aR, Un AC: 690 V, Un DC: 700 V, DC according to UL",15.49,"ΤΕΜ",1,"LP",5,"3NC2220"]
["3ND2122","LV HRC fuse element, NH1, In: 63 A, aM, Un AC: 690 V, Un DC: 400 V, Front indicator, live grip lugs",42.6,"ΤΕΜ",1,"LP",3,"3ND2122"]
["3NE1225-4D","PV fuse link, with blade contacts, NH1L, In: 200 A, gPV, Un DC: 1000 V, front indicator",275.26,"ΤΕΜ",1,"LP",2,"3NE12254D"]
["3NE4124","SITOR fuse link, with blade contacts, NH0, In: 160 A, aR, Un AC: 1000 V, Un DC: 440 V, front indicator",67.150000000000006,"ΤΕΜ",1,"LP",3,"3NE4124"]
["3NE8224-0MK","SITOR fuse link, with blade contacts, NH1, In: 160 A, aR, Un AC: 690 V, Un DC: 440 V, front indicator",67.22,"ΤΕΜ",1,"LP",3,"3NE82240MK"]
["3NH3220","LV HRC fuse base Sz. 1, 1-pole 250 A 690 V (1000 V) Double busbar terminal",49.19,"ΤΕΜ",1,"LP",3,"3NH3220"]
["3NJ4153-3BF01","Fuse switch disconnector 3-pole selectable, new design for protection of transformers on the secondary side up to 500 kVA for LV HRC fuses GTR 722 A max., 400 V AC, and NH3 Disconnecting blade up to 1000 A",1069.03,"ΤΕΜ",1,"LP",1,"3NJ41533BF01"]
["3NJ6213-1AA00-2DG4","Switch disconnector with fuses In-line design, pluggable NH1 250 A, 3-pole Standard switching capacity S manual operation without auxiliary switch 1 current transformer on 1 ammeter, Bimetal 250/5 A, Cl. 1 1, 2-fold overload",1363.57,"ΤΕΜ",1,"LP",1,"3NJ62131AA002DG4"]
["3NJ6234-2AA00-0AA0","Switch disconnector with fuses In-line design, pluggable NH3 630 A, 4-pole Standard switching capacity S Motor drive, without auxiliary switch without current transformer without ammeter",5560.66,"ΤΕΜ",1,"LP",1,"3NJ62342AA000AA0"]
["3NJ6920-3BE11","accessory for Switch disconnector with fuses In-line design, pluggable current transformer 150/1 A, Cl. 1, 2.5 VA",82.22,"ΤΕΜ",1,"LP",1,"3NJ69203BE11"]
["3NJ6933-4BB00","accessory for Switch disconnector with fuses In-line design, plug-in, NH1 Front panel for 3NJ6213-1, 3NJ6213-3, 3NJ6214-1",99.300000000000011,"ΤΕΜ",1,"LP",1,"3NJ69334BB00"]
["3NP1133-1BC11","SENTRON, Fuse switch disconnector 3NP1, 3-pole, NH00, 160 A, for Busbar system 8US 60 mm, flat terminal, Fuse monitoring: electromechanical, Cover level 32/70 mm",223.08,"ΤΕΜ",1,"LP",1,"3NP11331BC11"]
["3NP1143-1JC23","SENTRON, Fuse switch disconnector 3NP1, 3-pole, NH1, 250 A, for Rittal busbar system 60 mm, Box terminal, Fuse monitoring: electronic EFM20, Cover level 32/70 mm",487.08,"ΤΕΜ",1,"LP",1,"3NP11431JC23"]
["3NP1163-1DA13","SENTRON, Fuse switch disconnector 3NP1, 3-pole, NH3, 630 A, for assembly and installation on mounting plate, flat terminal, Fuse monitoring: electronic EFM20, Cover level 70 mm",500.28,"ΤΕΜ",1,"LP",1,"3NP11631DA13"]
["3NP1943-1BG40","Auxiliary conductor connection 0.25 - 1 mm2, for size NH1 with Box terminal, accessory for fuse switch disconnector 3NP1 Contains 3 connections",11.38,"ΤΕΜ",1,"LP",1,"3NP19431BG40"]
["3NP5460-0CA10","SENTRON, Fuse switch disconnector 3NP5, 3-pole, NH3, 630 A, for assembly and installation on mounting plate, with High-speed closing, screw terminal, Auxiliary switch on switch disconnector: 1 NO+1 NC",725.61,"ΤΕΜ",1,"LP",1,"3NP54600CA10"]
["3NW1300-0HG","SENTRON, cylindrical fuse link, Class CC, 30 A, time-lag, Un AC: 600 V, respect national installation rules!",30.82,"ΤΕΜ",1,"LP",10,"3NW13000HG"]
["3NW6212-1","SENTRON, cylindrical fuse link, 22x58 mm, 32 A, gG, Un AC: 690 V",5.76,"ΤΕΜ",1,"LP",10,"3NW62121"]
["3NW7314","SENTRON, cylindrical fuse holder, 8x32 mm, 1-pole, In: 20 A, Un AC: 400 V, LED signal detector",10,"ΤΕΜ",1,"LP",1,"3NW7314"]
["3NY1210","Accessory for switch 3NP5260 Assembly kit with molded plastic cover 300 x 220 mm",58.22,"ΤΕΜ",1,"LP",1,"3NY1210"]
["3RA1953-2B","Set of link rails between delta contactor 3RT1.5 and star (wye) contactor 3RT1.5 phase swapping output side , including neutral bridge",336,"ΤΕΜ",1,"CP",1,"3RA19532B"]
["3RA2110-1AA15-1FB4","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S00 1.10...1.60 A 24 V DC screw terminal for installation on standard mounting rail (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO (contactor) with diode (integrated)",110,"ΤΕΜ",1,"CP",1,"3RA21101AA151FB4"]
["3RA2110-1KE17-1BB4","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S00 9.00...12.5 A 24 V DC Spring-type terminal for installation on standard mounting rail Type of coordination 1, Iq = 150 kA 1 NO (contactor)",122,"ΤΕΜ",1,"CP",1,"3RA21101KE171BB4"]
["3RA2120-1HD24-0BB4","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S0 5.50...8.00 A 24 V DC screw terminal for 60 mm busbar systems (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO+1 NC (contactor)",189,"ΤΕΜ",1,"CP",1,"3RA21201HD240BB4"]
["3RA2125-1HH24-0FB4","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S0 5.50...8.00 A 24 V DC Spring-type terminal for 60 mm busbar systems (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO+1 NC (contactor) with diode combination plugged in at the front",224,"ΤΕΜ",1,"CP",1,"3RA21251HH240FB4"]
["3RA2130-4VA36-0AP0","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S2 35...45 A 230 V AC, 50 Hz screw terminal for installation on standard mounting rail (also fulfills type of coordination 1) Type of coordination 2, Iq = 100 kA 1 NO+1 NC (contactor)",376,"ΤΕΜ",1,"CP",1,"3RA21304VA360AP0"]
["3RA2210-0FH15-2BB4","Load feeder fuseless, Reversing duty 400 V AC, Size S00 0.35...0.50 A 24 V DC Spring-type terminal for 60 mm busbar systems (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NC (contactor)",198,"ΤΕΜ",1,"CP",1,"3RA22100FH152BB4"]
["3RA2220-1GF24-0AP0","Load feeder fuseless, Reversing duty 400 V AC, Size S0 4.50...6.30 A 230 V AC Spring-type terminal for installation on standard mounting rail with standard mounting rail adapter (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO+1 NC (contactor)",206,"ΤΕΜ",1,"CP",1,"3RA22201GF240AP0"]
["3RA2220-1JD24-0BB4","Load feeder fuseless, Reversing duty 400 V AC, Size S0 7.00...10.0 A 24 V DC screw terminal for 60 mm busbar systems (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO+1 NC (contactor)",320,"ΤΕΜ",1,"CP",1,"3RA22201JD240BB4"]
["3RA2316-8XB37-1CH0","Reversing contactor assembly AC-3,4 kW/400 V,AC48 V,50/60 Hz 3-pole, Size S00 screw terminal electrical and mechanical interlock 2 x auxiliary switch plugged on 2 x varistor plugged on",146,"ΤΕΜ",1,"CP",1,"3RA23168XB371CH0"]
["3RA2318-8XB30-2BB4","Reversing contactor assembly AC-3, 7.5 kW/400 V, 24 V DC 3-pole, Size S00 Spring-type terminal electrical and mechanical interlock",175,"ΤΕΜ",1,"CP",1,"3RA23188XB302BB4"]
["3RA2337-8XB30-1AK6","Reversing contactor assembly AC-3, 30 kW/400 V 110 V AC 50 Hz/120 V 60 Hz, 3-pole Size S2, screw terminal electrical and mechanical Interlock 2 NO integrated",452,"ΤΕΜ",1,"CP",1,"3RA23378XB301AK6"]
["3RA2417-8XF31-1AB0","Contactor assembly for star-delta (wye-delta) start AC-3, 11 kW/400 V, 24 V AC 50/60 Hz, 3-pole, Size S00 screw terminals electrical and mechanical interlock 3 NO integrated",291,"ΤΕΜ",1,"CP",1,"3RA24178XF311AB0"]
["3RA2712-1BA00","Function module for AS-i, Reversing start, screw terminal, Installation on contactors 3RT2 Communication-capable contactor required",126,"ΤΕΜ",1,"CP",1,"3RA27121BA00"]
["3RA2934-2B","Mechanical interlocking can be mounted on the side for contactors S2/S3",10.3,"ΤΕΜ",1,"CP",1,"3RA29342B"]
["3RA6120-2EP33","SIRIUS Compact load feeder DOL starter 690 V 110...240 V AC/DC 50...60 Hz 8...32 A IP20 Connection main circuit: plug-in, without terminals Connection auxiliary circuit: Spring-type terminal",665,"ΤΕΜ",1,"CP",1,"3RA61202EP33"]
["3RA6250-1CB32","SIRIUS Compact load feeder Reversing starter 690 V 24 V AC/DC 50...60 Hz 1...4 A IP20 Connection main circuit: Screw terminal Connection control circuit: screw terminal",732,"ΤΕΜ",1,"CP",1,"3RA62501CB32"]
["3RA6932-0A","Connecting cable, 10-pole 8 mm",17.900000000000002,"ΤΕΜ",1,"CP",5,"3RA69320A"]
["3RB2987-2B","Connecting cable 0.1 m for 3RB22/23/24 Size S00...S12",12,"ΤΕΜ",1,"CP",1,"3RB29872B"]
["3RB3046-2XX1","Overload relay 32...115 A Electronic For motor protection Size S3, Class 20E Stand-alone installation Main circuit: Straight-through transformer Auxiliary circuit: Spring-type terminal Manual-Automatic-Reset",209,"ΤΕΜ",1,"CP",1,"3RB30462XX1"]
["3RF2150-2AA06","Semiconductor relay, 1-phase 3RF2 Overall width 22.5 mm, 50 A 48-600 V / 24 V DC Spring-type terminal",67.900000000000006,"ΤΕΜ",1,"CP",1,"3RF21502AA06"]
["3RF2320-1AA04","Solid-state contactor 1-phase 3RF2 AC 51 / 20 A / 40 Β°C 48-460 V / 24 V DC screw terminal",67.099999999999994,"ΤΕΜ",1,"CP",1,"3RF23201AA04"]
["3RF2340-1AA06","Solid-state contactor 1-phase 3RF2 AC 51 / 40 A / 40 Β°C 48-600 V / 24 V DC screw terminal",99.1,"ΤΕΜ",1,"CP",1,"3RF23401AA06"]
["3RF2390-3AA22","Solid-state contactor 1-phase 3RF2 AC 51 / 88 A / 40 Β°C 24-230 V / 110-230 V AC Ring cable connection Phased-out product, no successor available!",283,"ΤΕΜ",1,"CP",1,"3RF23903AA22"]
["3RF2900-0SA88","Spare part DIN rail adapter for 3RF23 22.5 mm wide",2.8,"ΤΕΜ",1,"CP",10,"3RF29000SA88"]
["3RF3416-1BB04","Solid-state contactor 3-phase 3RF3 AC 53 / 16 A / 40 Β°C 48-480 V / 24 V DC 2-phase controlled Instantaneous switching screw terminal",196,"ΤΕΜ",1,"CP",1,"3RF34161BB04"]
["3RH2122-1AP00","Contactor relay, 2 NO + 2 NC, 230 V AC, 50 / 60 Hz, Size S00, screw terminal",30.3,"ΤΕΜ",1,"CP",1,"3RH21221AP00"]
["3RH2122-2XF40-0LA2","Contactor relay for railway 2 NO + 2 NC, DC 72-125V, 0,7...1,25*US, with integrated varistor Size S00, Spring-type terminal suitable for PLC outputs",55.300000000000004,"ΤΕΜ",1,"CP",1,"3RH21222XF400LA2"]
["3RH2140-1AN20","Contactor relay, 4 NO, 220 V AC, 50 / 60 Hz, Size S00, screw terminal",30.3,"ΤΕΜ",1,"CP",1,"3RH21401AN20"]
["3RH2140-2JC40","Coupling contactor relay, 4 NO, 30 V DC, 0.7 ... 1.25* US, with integrated diode, Size S00, Spring-type terminal suitable for PLC outputs",40,"ΤΕΜ",1,"CP",1,"3RH21402JC40"]
["3RH2353-1CP00-0KA0","Contactor relay, 5 NO + 3 NC, 230 V AC, 50 / 60 Hz, Size S00, screw terminal, 2 NO + 2 NC basic unit / EN Varistor plugged on",60.300000000000004,"ΤΕΜ",1,"CP",1,"3RH23531CP000KA0"]
["3RH2440-1AB00","Contactor relay, latched, 4 NO, 24 V AC, 50 / 60 Hz, Size S00, screw terminal",105,"ΤΕΜ",1,"CP",1,"3RH24401AB00"]
["3RH2911-4HA30","Auxiliary switch on the front, 3 NO Current path 1 NO, 1 NO, 1 NO for 3RH and 3RT Ring cable lug connection .3/.4, .3/.4, .3/.4",12.4,"ΤΕΜ",1,"CP",1,"3RH29114HA30"]
["3RK1301-0CB13-0AA2","F-DS1E-X for ET 200S Fail-safe DOL starter Setting range 2.4...16 A Mechanical switching Electronic protection AC-3, up to 7.5 kW / 400 V expandable for brake control module for 2DI control module",912,"ΤΕΜ",1,"CP",1,"3RK13010CB130AA2"]
["3RK1308-0CA00-0CP0","Fail-safe direct-on-line starter High Feature; Electronic switching; Electronic overload protection up to 0.09 kW / 400 V; Adjustment range 0.1 .. 0.4 A; PROFIenergy; Option: 3DI/LC module",465,"ΤΕΜ",1,"CP",1,"3RK13080CA000CP0"]
["3RK1315-6KS41-3AA3","SIRIUS motor starter M200D AS-i Communication: AS-Interface Reversing starter Basic Mechanical switching AC-3, 0.75KW / 400 V 0.15 A...2.00 A Electronic overload protection Thermistor: THERMOCLICK / PTC with brake contact 400 V AC 2DI AS-i + 2DI / 1DO on device Han Q4/2 - Han Q8/0 with manual on-site operation and key-operated switch",1092,"ΤΕΜ",1,"CP",1,"3RK13156KS413AA3"]
["3RK1395-6KS71-2AD0","SIRIUS motor starter M200D Technology module DOL starter Electronic switching AC-3, 0.75KW / 400 V 0.15 A...2.00 A Electronic overload protection Thermistor: THERMOCLICK / PTC without brake contact 4 DI / 2 DO Han Q4/2 - Han Q8/0 with manual on-site operation and key-operated switch via communication module 3RK1305* can be used on PROFIBUS or PROFINET",1117,"ΤΕΜ",1,"CP",1,"3RK13956KS712AD0"]
["3RK1405-0BQ00-0AA3","ASIsafe compact module K60F digital safety, 2 F-DI/2 DQ, IP67 2 x input for mechanical sensors 2 x standard output 24 V DC Output supply from U_ASI 4 x M12 socket Mounting plate 3RK1901-0CA00 must be ordered separately",353,"ΤΕΜ",1,"CP",1,"3RK14050BQ000AA3"]
["3RK1902-0CB00","Connector set, infeed 6 x 4 mm2, 9-pole, complete with PG16 cable entry",49.1,"ΤΕΜ",1,"CP",1,"3RK19020CB00"]
["3RK1903-3EC10","65 mm terminal module for ET 200S inverter power module IPM25 FS A without supply line connection",360,"ΤΕΜ",1,"CP",1,"3RK19033EC10"]
["3RK2400-1CE01-0AA2","AS-i SlimLine module Phased-out product !!! For further information, please contact our sales department S45 digital, A/B slave 4 DI/4 DQ, IP20 4 x inputs for 3-wire sensor 4 x output, 2 A, 24 V DC maximal 4 A for all outputs Screw terminals Overall width 45 mm",328,"ΤΕΜ",1,"CP",1,"3RK24001CE010AA2"]
["3RK4324-3BR54-1BC0","SIRIUS MCU motor starter Enclosure degree of protection IP54 plastic Communication AS-Interface electromechanically switching Short-circuit protection with circuit breaker Reversing starter Brake without Performance class 0.8 A Motor circuit breaker with bi-metal thermal with manual operation Connection power M screw connection Special variant new design A/B slave AS-i SPEC V2.1 Sensor-actuator 1x AS-i 1xDI/DO Supply sensor U-AUX",1276,"ΤΕΜ",1,"CP",1,"3RK43243BR541BC0"]
["3RK4340-3LR51-1BA0","SIRIUS MCU motor starter Enclosure degree of protection IP55 plastic Communication without electromechanically switching Short-circuit protection with circuit breaker Reversing starter Brake without Performance class 6.30 A Motor circuit breaker with bi-metal thermal Manual operation without Connection power M screw connection Standard product",681,"ΤΕΜ",1,"CP",1,"3RK43403LR511BA0"]
["3RM1101-1AA04","Fail-safe direct starter, 3RM1, 500 V, 0 - 0.12 kW, 0.1 - 0.5 A, 24 V DC, screw terminals",186,"ΤΕΜ",1,"CP",1,"3RM11011AA04"]
["3RN2000-1AW30","Thermistor motor protection relay Compact evaluation unit, 17.5 mm enclosure, screw terminals, 1 changeover contact, US = 24 V-240 V AC/DC, Auto RESET, suitable for bimetallic switch, supply =output voltage, 1 LED (tripped)",53,"ΤΕΜ",1,"CP",1,"3RN20001AW30"]
["3RN2012-1BA30","Thermistor motor protection relay Standard evaluation unit 22.5 mm enclosure screw terminal 2 change-over contacts US = 24 V AC/DC Manual/Auto/Remote reset with ATEX approval 2 LEDs (READY/TRIPPED) galvanic isolation Test/reset button Wire break monitoring Short circuit monitoring non-volatile",114,"ΤΕΜ",1,"CP",1,"3RN20121BA30"]
["3RP1576-1NM20","Timing relay, electronic Phased-out product !!! For further information, please contact our sales department with star-delta (wye-delta) function 1 NO contact, delayed 1 NO contact, instantaneous 1 time range 3...60 s 200-240 V AC and 380-440 V AC screw terminal",141,"ΤΕΜ",1,"CP",1,"3RP15761NM20"]
["3RP2560-1SW30","Timing relay, electronic with star-delta (wye-delta) function 1-20 s, Overshoot time 30-600 s 3 NO contacts with common potential 12-240 V AC/DC at 50/60 Hz AC screw terminal 0.85 ...1.1 US",118,"ΤΕΜ",1,"CP",1,"3RP25601SW30"]
["3RR2441-2AA40","Current monitoring relay for IO-Link, can be mounted to Contactor 3RT2, Size S00 Apparant/active current monitoring 1.6-16 A, 20-400 Hz, 3-phase Supply voltage 24 V DC 1 change-over contact Monitoring for Current overshoot and undershoot Current asymmetry Phase failure, Cable break Phase sequence, Residual current Blocking current, Switching cycle and Operating hours counter Warning and alarm thresholds Auto-reset or manual reset ON delay 0-9999.9 s OFF delay 0-9999.9 s Reclosing delay 0-300 min spring-type connection system",244,"ΤΕΜ",1,"CP",1,"3RR24412AA40"]
["3RS1101-1CK30","Temperature monitoring relay Thermocouple type K, overshoot 1 threshold value, Width 22.5 mm 0 Β°C to 600 Β°C 110-120/220-240 V AC 1 NO + 1 NC, quiescent current principle screw terminal",158,"ΤΕΜ",1,"CP",1,"3RS11011CK30"]
["3RS1800-2HW00","!!! Phased-out product !!! The preferred successor is 3RQ2000-2CW00. Coupling relays in industrial enclosure 3 change-over contacts Wide voltage range 24 V to 240 V AC/DC Spring-type terminal",78.899999999999991,"ΤΕΜ",1,"CP",1,"3RS18002HW00"]
["3RT1054-6AM36","Power contactor, AC-3 115 A, 55 kW / 400 V AC (50-60 Hz) / DC operation 200-220 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, Size S6 Busbar connections Drive: conventional screw terminal",365,"ΤΕΜ",1,"CP",1,"3RT10546AM36"]
["3RT1054-6AU36","Power contactor, AC-3 115 A, 55 kW / 400 V AC (50-60 Hz) / DC operation 240-277 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, Size S6 Busbar connections Drive: conventional screw terminal",365,"ΤΕΜ",1,"CP",1,"3RT10546AU36"]
["3RT1056-6AF36-3PA0","Power contactor, AC-3 185 A, 90 kW / 400 V AC (50-60 Hz) / DC operation UC 110-127 V Auxiliary contacts 2 NO + 2 NC lateral, permanently mounted 3-pole, Size S6 Busbar connections Drive: conventional",538,"ΤΕΜ",1,"CP",1,"3RT10566AF363PA0"]
["3RT1065-6NF36","Power contactor, AC-3 265 A, 132 kW / 400 V AC (50-60 Hz) / DC operation 96-127 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, Size S10 Busbar connections Drive: electronic with PLC interface 24 V DC screw terminal",977,"ΤΕΜ",1,"CP",1,"3RT10656NF36"]
["3RT1076-2AT36","Power contactor, AC-3 500 A, 250 kW / 400 V AC (50-60 Hz) / DC 575-600 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, size S12 Busbar connections Operating mechanism: conventional Spring-type terminals",1579,"ΤΕΜ",1,"CP",1,"3RT10762AT36"]
["3RT1266-6NB36","Vacuum contactor, AC-3 300 A, 160 kW / 400 V AC (50-60 Hz) / DC operation 21-27.3 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, Size S10 Busbar connections Drive: electronic with PLC interface 24 V DC",1807,"ΤΕΜ",1,"CP",1,"3RT12666NB36"]
["3RT1456-6AP38-0PA5","Contactor, AC-1, 275 A/690 V/40 Β°C, S6, 3-pole, 220-240 V AC/DC, with varistor, 2 NO+2 NC, encapsulated, Connection rail/ screw terminal",433,"ΤΕΜ",1,"CP",1,"3RT14566AP380PA5"]
["3RT1916-4KA6","Soldering pin adapter for contactors with mounted 4-pole auxiliary switch block for 3RT101.1. with 3.8 mm long soldering pins consists of 4 adapters for 1 contactor !!! Phased-out product !!! Successor is SIRIUS 3RT2",11.2,"ΤΕΜ",1,"CP",4,"3RT19164KA6"]
["3RT1956-4EA2","Terminal cover on box terminal from 3RT1, 3RB2, 3RW405, 3RW442, 3RW443, size S6",13,"ΤΕΜ",1,"CP",1,"3RT19564EA2"]
["3RT1966-7B","Arc chute for 3RT1466",184,"ΤΕΜ",1,"CP",1,"3RT19667B"]
["3RT2015-1AV02","Power contactor, AC-3 7 A, 3 kW / 400 V 1 NC, 400 V AC, 50 / 60 Hz 3-pole, Size S00 screw terminal",29.3,"ΤΕΜ",1,"CP",1,"3RT20151AV02"]
["3RT2015-1VB42","power contactor, AC-3 7 A, 3 kW / 400 V 1 NC, 24 V DC 0.85-1.85* US, with diode integrated, 3-pole, size S00, screw terminal not expandable with auxiliary switch",36.6,"ΤΕΜ",1,"CP",1,"3RT20151VB42"]
["3RT2015-2BW42","Power contactor, AC-3 7 A, 3 kW / 400 V 1 NC, 48 V DC 3-pole, Size S00 Spring-type terminal",31.1,"ΤΕΜ",1,"CP",1,"3RT20152BW42"]
["3RT2016-1BB41-0CC0","Power contactor, AC-3 9 A, 4 kW / 400 V 1 NO, 24 V DC communication-capable, 3-pole, Size S00, screw terminal",36,"ΤΕΜ",1,"CP",1,"3RT20161BB410CC0"]
["3RT2016-2AP02-1AA0","power contactor, AC-3 9 A 4 kW / 400 V 1 NC, 230 V AC, 50/60 Hz 3-pole, Size S00 Spring-type terminal upright mounting position",29.200000000000003,"ΤΕΜ",1,"CP",1,"3RT20162AP021AA0"]
["3RT2017-1AP04-3MA0","Power contactor, AC-3 12 A, 5.5 kW / 400 V 2 NO + 2 NC, 230 V AC, 50 / 60 Hz 3-pole, Size S00 Screw terminal Captive auxiliary switch",47.300000000000004,"ΤΕΜ",1,"CP",1,"3RT20171AP043MA0"]
["3RT2017-2FB41-1AA0","power contactor, AC-3 12 A, 5.5 kW / 400 V 1 NO, 24 V DC with diode integrated, 3-pole Size S00, Spring-type terminal upright mounting position",44.300000000000004,"ΤΕΜ",1,"CP",1,"3RT20172FB411AA0"]
["3RT2017-4BB42","power contactor, AC-3 12 A, 5.5 kW / 400 V 1 NC, 24 V DC 3-pole, Size S00 ring cable lug connection",36.9,"ΤΕΜ",1,"CP",1,"3RT20174BB42"]
["3RT2018-1FB41","Power contactor, AC-3 16 A, 7.5 kW / 400 V 1 NO, 24 V DC with diode integrated, 3-pole, Size S00, screw terminals",73.899999999999991,"ΤΕΜ",1,"CP",1,"3RT20181FB41"]
["3RT2023-1AT60","power contactor, AC-3 9 A, 4 kW / 400 V 1 NO + 1 NC, 600 V AC, 60 Hz 3-pole, Size S0 screw terminal",33.700000000000003,"ΤΕΜ",1,"CP",1,"3RT20231AT60"]
["3RT2023-2AG24","power contactor, AC-3 9 A, 4 kW / 400 V 2 NO + 2 NC, 110 V AC 50 / 60 Hz, 3-pole Size S0, Spring-type terminal Removable auxiliary switch",43.1,"ΤΕΜ",1,"CP",1,"3RT20232AG24"]
["3RT2024-1FB40","power contactor, AC-3 12 A, 5.5 kW / 400 V 1 NO + 1 NC, 24 V DC with plugged-in diode combination, 3-pole Size S0, screw terminal",81.5,"ΤΕΜ",1,"CP",1,"3RT20241FB40"]
["3RT2025-1AD04","power contactor, AC-3 17 A, 7.5 kW / 400 V 2 NO + 2 NC, 42 V AC, 50 Hz, 3-pole, Size S0 screw terminal Removable auxiliary switch",62.2,"ΤΕΜ",1,"CP",1,"3RT20251AD04"]
["3RT2026-1AC20","power contactor, AC-3 25 A, 11 kW / 400 V 1 NO + 1 NC, 24 V AC, 50 / 60 Hz, 3-pole, Size S0, screw terminal",64.099999999999994,"ΤΕΜ",1,"CP",1,"3RT20261AC20"]
["3RT2026-2AD00","Power contactor, AC-3 25 A, 11 kW / 400 V 1 NO + 1 NC, 42 V AC, 50 Hz, 3-pole, Size S0 Spring-type terminal",67.099999999999994,"ΤΕΜ",1,"CP",1,"3RT20262AD00"]
["3RT2026-4KB40","power contactor, AC-3 25 A, 11 kW / 400 V 1 NO + 1 NC 24 V DC, DC 0.7-1.25* US, with integrated varistor 3-pole, size S0 ring cable lug connection suitable for PLC outputs not expandable with auxiliary switch",110,"ΤΕΜ",1,"CP",1,"3RT20264KB40"]
["3RT2027-2FB44-3MA0","Power contactor, AC-3 32 A, 15 kW / 400 V 2 NO + 2 NC, 24 V DC with plugged-in diode combination, 3-pole Size S0 Spring type terminal Captive auxiliary switch",162,"ΤΕΜ",1,"CP",1,"3RT20272FB443MA0"]
["3RT2028-1BG40","Power contactor, AC-3 38 A, 18.5 kW / 400 V 1 NO + 1 NC, 125 V DC 3-pole, size S0 screw terminals",149,"ΤΕΜ",1,"CP",1,"3RT20281BG40"]
["3RT2035-1AR64","power contactor, AC-3 40 A, 18.5 kW / 400 V 2 NO + 2 NC, 400 V AC AC (50-60 Hz) / DC operation 3-pole, Size S2, screw terminal",128,"ΤΕΜ",1,"CP",1,"3RT20351AR64"]
["3RT2035-1NB34","power contactor, AC-3 40 A, 18.5 kW / 400 V 2 NO + 2 NC, AC / DC 20-33 V, with varistor, 3-pole, Size S2, screw terminal",181,"ΤΕΜ",1,"CP",1,"3RT20351NB34"]
["3RT2036-3AF04","power contactor, AC-3 50 A, 22 kW / 400 V 2 NO + 2 NC, 110 V AC, 50 Hz 3-pole, Size S2, Spring-type terminal",148,"ΤΕΜ",1,"CP",1,"3RT20363AF04"]
["3RT2037-1AN20","Power contactor, AC-3 65 A, 30 kW / 400 V 1 NO + 1 NC, 220 V AC 50/60 Hz, 3-pole Size S2, screw terminals",189,"ΤΕΜ",1,"CP",1,"3RT20371AN20"]
["3RT2038-1AK64","Contactor, AC-3, 37 kW / 400 V, 2 NO + 2 NC, 110 V AC, 50 Hz / 120 V, 60 Hz, 3-pole, Size S2, screw terminal",252,"ΤΕΜ",1,"CP",1,"3RT20381AK64"]
["3RT2045-1AK64-3MA0","Power contactor, AC-3 80 A, 37 kW / 400 V 2 NO + 2 NC, AC 110 V/50 Hz 120 V/60 Hz 3-pole, 3S, Size S3 screw terminal Captive auxiliary switch",252,"ΤΕΜ",1,"CP",1,"3RT20451AK643MA0"]
["3RT2046-1AP04","power contactor, AC-3 95 A, 45 kW / 400 V 2 NO + 2 NC, 230 V AC, 50 Hz 3-pole, 3 NO, Size S3 screw terminal",297,"ΤΕΜ",1,"CP",1,"3RT20461AP04"]
["3RT2047-3NP30","Power contactor, AC-3 115 A, 55 kW /  400 V 1 NO + 1 NC, 175-280 V AC/DC 3-pole, 3 NO, Size S3 Spring-type terminals integrated varistor",397,"ΤΕΜ",1,"CP",1,"3RT20473NP30"]
["3RT2325-2AG20","Contactor, AC-1, 35 A/400 V/40 Β°C, S0, 4-pole, 110 V AC, 50/60 Hz, 1 NO+1 NC, Spring-type terminal",55,"ΤΕΜ",1,"CP",1,"3RT23252AG20"]
["3RT2327-2AP00","Contactor, AC-1, 50 A/400 V/40 Β°C, S0, 4-pole, 230 V AC/50 Hz, 1 NO+1 NC, Spring-type terminal",108,"ΤΕΜ",1,"CP",1,"3RT23272AP00"]
["3RT2448-1NP30","Contactor, AC-1, 160 A/690 V/40 Β°C, S3, 3-pole, 175-280 V AC/DC, with varistor, 1 NO+1 NC, box terminal/screw terminal",364,"ΤΕΜ",1,"CP",1,"3RT24481NP30"]
["3RT2516-2AF00","Contactor, 2 NO + 2 NC, AC-3, 4 kW 110 V AC, 50/60 Hz, 4-pole, 2 NO+ 2 NC, Size S00, spring-type terminal",29.900000000000002,"ΤΕΜ",1,"CP",1,"3RT25162AF00"]
["3RT2526-1BM40","Power contactor, AC-3 25 A, 11 kW / 400 V 2 NO + 2 NC 220 V DC, 50 Hz 4-pole size S0 screw terminals 1 NO + 1 NC integrated",130,"ΤΕΜ",1,"CP",1,"3RT25261BM40"]
["3RT2627-1AC25","Capacitor contactor, AC-6b 25 kVAr, / 400 V 1 NO + 2 NC, 24 V AC, 50/60 Hz 3-pole, Size S0 screw terminal",113,"ΤΕΜ",1,"CP",1,"3RT26271AC25"]
["3RT2924-5AH01","Magnet coil for contactors 7.5 kW 48 V AC, 50 Hz, for motor contactors, Size S0, Screw terminal",19.399999999999999,"ΤΕΜ",1,"CP",1,"3RT29245AH01"]
["3RT2926-4RA12","Coil connection module for motor contactors, Size S0, connection from top Spring-type terminal",4.2300000000000004,"ΤΕΜ",1,"CP",1,"3RT29264RA12"]
["3RT2944-5AD21","Magnet coil for contactor S3, 42 V AC, 50 / 60 Hz,",30.6,"ΤΕΜ",1,"CP",1,"3RT29445AD21"]
["3RU2116-1FB0","Overload relay 3.5...5.0 A Thermal For motor protection Size S00, Class 10 Contactor mounting Main circuit: Screw Auxiliary circuit: Screw Manual-Automatic-Reset",43.4,"ΤΕΜ",1,"CP",1,"3RU21161FB0"]
["3RU2126-4DC1","Overload relay 20...25 A Thermal For motor protection Size S0, Class 10 Stand-alone installation Main circuit: Spring-type terminal Auxiliary circuit: spring-type terminal Manual-Automatic-Reset",53.6,"ΤΕΜ",1,"CP",1,"3RU21264DC1"]
["3RU2126-4PJ0","Overload relay 30...36 A Thermal For motor protection Size S0, Class 10 Contactor mounting Main circuit: Ring cable lug Auxiliary circuit: ring cable lug Manual-Automatic-Reset",64.899999999999991,"ΤΕΜ",1,"CP",1,"3RU21264PJ0"]
["3RV1342-4JC10-0FB0","Circuit breaker size S3 For starter combination Rated current 63 A Short-circuit release 819 A Screw terminal Increased switching capacity ABB",476,"ΤΕΜ",1,"CP",1,"3RV13424JC100FB0"]
["3RV1923-1DA01","Cast aluminum surface mounting enclosure Degree of protection IP65 72 mm installation width with PE terminal for circuit breaker Size S0",56.6,"ΤΕΜ",1,"CP",1,"3RV19231DA01"]
["3RV1991-1AA0","Auxiliary switch 250 V AC/DC 1 signaling changeover switch 1 tripped signal for size 3RV1. 5, 6, 7, 8",41.5,"ΤΕΜ",1,"CP",1,"3RV19911AA0"]
["3RV2011-1CA10","Circuit breaker size S00 for motor protection, CLASS 10 A-release 1.8...2.5 A N-release 33 A screw terminal Standard switching capacity",50.4,"ΤΕΜ",1,"CP",1,"3RV20111CA10"]
["3RV2021-0JA20-0BA0","Special type Circuit breaker size S0 for motor protection, CLASS 10 A-release 0.7...1 A N-release 13 A Spring-type terminal Standard switching capacity Ambient temperature -50 Β°C 500 switching cycles",77.599999999999994,"ΤΕΜ",1,"CP",1,"3RV20210JA200BA0"]
["3RV2021-4EA15-0BA0","Special type Circuit breaker size S0 for motor protection, CLASS 10 A-release 27...32 A N-release 400 A screw terminal Standard switching capacity with transverse auxiliary switches 1 NO+1 NC Ambient temperature -50 Β°C 500 switching cycles",129,"ΤΕΜ",1,"CP",1,"3RV20214EA150BA0"]
["3RV2041-4RA15","Circuit breaker size S3 for motor protection, CLASS 10 A-release 65...84 A N-release 1170 A screw terminal Standard switching capacity with transverse auxiliary switches 1 NO+1 NC",245,"ΤΕΜ",1,"CP",1,"3RV20414RA15"]
["3RV2311-0HC20","Circuit breaker size S00 for starter combination Rated current 0.8 A N-release 10 A Spring-type terminal Standard switching capacity",44.1,"ΤΕΜ",1,"CP",1,"3RV23110HC20"]
["3RV2321-4EC20","Circuit breaker size S0 for starter combination Rated current 32 A N-release 400 A Spring-type terminal Standard switching capacity",71.399999999999991,"ΤΕΜ",1,"CP",1,"3RV23214EC20"]
["3RV2341-4JC10","Circuit breaker size S3 for starter combination Rated current 63 A N-release 819 A screw terminal Standard switching capacity",186,"ΤΕΜ",1,"CP",1,"3RV23414JC10"]
["3RV2421-4AA20","Circuit breaker size S0 for transformer protection A-release 10...16 A N-release 286 A Spring-type terminal Standard switching capacity",64,"ΤΕΜ",1,"CP",1,"3RV24214AA20"]
["3RV2811-1ED10","Circuit breaker size S00 for transformer protection with approval circuit breaker UL 489, CSA C22.2 No.5-02 A-release 4 A N-release 82 A screw terminal Standard switching capacity",130,"ΤΕΜ",1,"CP",1,"3RV28111ED10"]
["3RV2928-1H","Terminal block type E according to UL 508 for circuit breaker Size S00/S0",12.299999999999999,"ΤΕΜ",1,"CP",1,"3RV29281H"]
["3RW4028-2BB04","SIRIUS soft starter S0 38 A, 18.5 kW/400 V, 40 Β°C 200-480 V AC, 24 V AC/DC spring-type terminals",698,"ΤΕΜ",1,"CP",1,"3RW40282BB04"]
["3RW4047-1BB14","SIRIUS soft starter S3 106 A, 55 kW/400 V, 40 Β°C 200-480 V AC, 110-230 V AC/DC Screw terminals",1352,"ΤΕΜ",1,"CP",1,"3RW40471BB14"]
["3RW4425-3BC35","SIRIUS soft starter Values at 575 V, 50 Β°C standard: 51 A, 40 hp Inside-delta: 88 A, 75 hp 400-600 V AC, 115 V AC spring-type terminals !!! Phased-out product !!! Successor is SIRIUS 3RW5, Preferred successor type is >>3RW5525-3HA16<<",2233,"ΤΕΜ",1,"CP",1,"3RW44253BC35"]
["3RW4435-6BC34","SIRIUS soft starter Values at 460 V, 50 Β°C standard: 117 A, 75 hp Inside-delta: 203 A, 150 hp 200-460 V AC, 115 V AC Screw terminals !!! Phased-out product !!!  Successor is SIRIUS 3RW5,  Preferred successor type is >>3RW5535-6HA14<<",3119,"ΤΕΜ",1,"CP",1,"3RW44356BC34"]
["3RW4456-6BC34","SIRIUS soft starter Values at 460 V, 50 Β°C standard: 693 A, 600 hp Inside-delta: 1200 A, 1050 hp 200-460 V AC, 115 V AC Screw terminals !!! Phased-out product !!!  Successor is SIRIUS 3RW5,  Preferred successor type is >>3RW5554-6HA14<<",13659,"ΤΕΜ",1,"CP",1,"3RW44566BC34"]
["3RW4457-6BC35","SIRIUS soft starter Values at 575 V, 50 Β°C standard: 780 A, 850 hp Inside-delta: 1351 A, 1500 hp 400-600 V AC, 115 V AC Screw terminals !!! Phased-out product !!!  Successor is SIRIUS 3RW5,  Preferred successor type is >>3RW5556-6HA16<<",16935,"ΤΕΜ",1,"CP",1,"3RW44576BC35"]
["3RW4747-6SC40","Control unit 230 V for 3RW44, Size 4 with screw terminals",816,"ΤΕΜ",1,"CP",1,"3RW47476SC40"]
["3RW5074-2TB15","SIRIUS soft starter 200-600 V 315 A, 110-250 V AC Spring-loaded terminals Thermistor input",3198,"ΤΕΜ",1,"CP",1,"3RW50742TB15"]
["3RW5076-2TB04","SIRIUS soft starter 200-480 V 470 A, 24 V AC/DC Spring-loaded terminals Thermistor input",3393,"ΤΕΜ",1,"CP",1,"3RW50762TB04"]
["3RW5217-3AC14","SIRIUS soft starter 200-480 V 38 A, 110-250 V AC spring-type terminals Analog output",1248,"ΤΕΜ",1,"CP",1,"3RW52173AC14"]
["3RW5234-2TC14","SIRIUS soft starter 200-480 V 113 A, 110-250 V AC spring-type terminals Thermistor input",2167,"ΤΕΜ",1,"CP",1,"3RW52342TC14"]
["3RW5246-2TC15","SIRIUS soft starter 200-600 V 370 A, 110-250 V AC spring-type terminals Thermistor input",6266,"ΤΕΜ",1,"CP",1,"3RW52462TC15"]
["3RW5248-6TC15","SIRIUS soft starter 200-600 V 570 A, 110-250 V AC Screw terminals Thermistor input",8294,"ΤΕΜ",1,"CP",1,"3RW52486TC15"]
["3RW5535-6HA14","SIRIUS soft starter 200-480 V 143 A, 110-250 V AC Screw terminals",3961,"ΤΕΜ",1,"CP",1,"3RW55356HA14"]
["3RW5548-6HF04","SIRIUS soft starter 200-480 V 570 A, 24 V AC/DC Screw terminals Fail-safe",12627,"ΤΕΜ",1,"CP",1,"3RW55486HF04"]
["3RW5558-6HA04","SIRIUS soft starter 200-480 V 1280 A, 24 V AC/DC Screw terminals",20424,"ΤΕΜ",1,"CP",1,"3RW55586HA04"]
["3RW5952-0SF05","Power semiconductor module 600 V, for 3RW52, 47 A",173,"ΤΕΜ",1,"CP",1,"3RW59520SF05"]
["3RX9513-0AA00","PSN130S 8 A 120 V/230 V AC IP20 Power supply unit 30 V, for AS-i without AS-i data decoupling IN: 120 V / 230 V AC OUT: 30 V DC, 8 A, IP20 with integrated Overload detection with signaling contact",512,"ΤΕΜ",1,"CP",1,"3RX95130AA00"]
["3SB2206-0LH01","Illuminated pushbutton, 16 mm, round, plastic, clear, pushbutton, raised, 1 NO, Lampholder W2 x 4.6 d,",23.3,"ΤΕΜ",1,"CP",1,"3SB22060LH01"]
["3SB2901-4RE","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with graphic symbol: 4",82.699999999999989,"ΤΕΜ",100,"CP",10,"3SB29014RE"]
["3SB2908-3AB","Protective cover, clear, Silicone for pushbutton unit with flat and raised pushbutton",3.41,"ΤΕΜ",1,"CP",1,"3SB29083AB"]
["3SE3934-5CB20","Pedal switch 2 change-over contacts 2-pedal, without protective cover",165,"ΤΕΜ",1,"CP",1,"3SE39345CB20"]
["3SE5000-0AE10-1AJ0","Actuator head for position switch 3SE52 Roller lever made of metal with Plastic roller 13 mm functional at -40 Β°C",11.299999999999999,"ΤΕΜ",1,"CP",1,"3SE50000AE101AJ0"]
["3SE5000-0AW42","Separate actuator with vertical fixing for position switch with tumbler with flange bushings made of stainless steel for 3SE5312../3SE5322.. and ASI 3SF13... and Position switch with separate actuator 3SE51/52 and ASI 3SF11../3SF12..",7.29,"ΤΕΜ",1,"CP",1,"3SE50000AW42"]
["3SE5112-0LH60","Position switch Metal enclosure 40 mm according to EN 50041 Device connection 1x (M20 x 1.5) 1 NO/2 NC quick action contacts Rotary actuator right/left adjustable with adjustable-length Metal lever 100 mm long and with positive fit (grid hole) and plastic roller 19 mm",56.2,"ΤΕΜ",1,"CP",1,"3SE51120LH60"]
["3SE5122-0CR01","Position switch Metal enclosure 56 mm wide, Device connection 3x (M20x 1.5), 1 NO/1 NC quick action contacts, Spring rod actuator, 142.5 mm total length, plunger plastic",43.9,"ΤΕΜ",1,"CP",1,"3SE51220CR01"]
["3SE5210-0AA00-1AG0","Cover for position switch Metal 3SE52, for Enclosure according to EN 50047, 31 mm Color yellow",4.12,"ΤΕΜ",1,"CP",1,"3SE52100AA001AG0"]
["3SE5212-0LB01","Position switch Metal enclosure 31 mm according to EN 50047 Device connection 1 x (M20 x 1.5) 1 NO/2 NC quick action contacts Plain plunger, stainless steel",33.200000000000003,"ΤΕΜ",1,"CP",1,"3SE52120LB01"]
["3SE5232-0LK15-1AL5","Position switch Plastic enclosure according to EN 50047, 31 mm Device connection 1 x (M20 x 1.5) 1 NO/2 NC quick action contacts Twist lever, 35 mm long right/left adjustable with plastic roller 19 mm customized Twist lever fixated clockwise at an angle: 70Β°",39.700000000000003,"ΤΕΜ",1,"CP",1,"3SE52320LK151AL5"]
["3SE5242-0HK21-1AJ0","Position switch Plastic 50 mm, Increased corrosion protection Device connection 2 x (M20 x 1.5) 1 NO/1 NC snap-action contacts twist lever metal lever with plastic roller 19 mm functional at -40 Β°C Shock and vibration test according to EN 61373, Category 1B",49.5,"ΤΕΜ",1,"CP",1,"3SE52420HK211AJ0"]
["3SE5322-1SB21","Safety position switch with tumbler Locking force 1300 N 5 directions of approaches Solenoid-locked Magnet voltage 24 V DC Monitoring actuator 2 NC/1 NO Monitoring magnet 2 NC/1 NO LED display yellow/green Supplied without actuator. Actuator 3SE5000-0AV. please order separately",229,"ΤΕΜ",1,"CP",1,"3SE53221SB21"]
["3SE5413-0CD23-1EA2","Position switch in compact design 30 mm wide with connection cable 2 m Snap-action contacts 1 NO+1 NC with roller plunger, plunger rotated by 90Β° Special customer version",46.1,"ΤΕΜ",1,"CP",1,"3SE54130CD231EA2"]
["3SF1324-1SD21-1BA1","Safety position switch with tumbler Locking force 1300 N 5 directions of approaches Plastic enclosure, M12 connector ASIsafe integrated Channel 1=actuator 1 NC Channel 2=magnet 1 NC spring-locked Auxiliary release on front Magnet voltage 24 V DC/AC Monitoring actuator 2 NC/1 NO Monitoring magnet 2 NC/1 NO The matching separate Actuator 3SE5000-0AV0 must be ordered separately",612,"ΤΕΜ",1,"CP",1,"3SF13241SD211BA1"]
["3SK1121-1CB41","SIRIUS safety relay Basic unit Advanced series with time delay 0.05-3 s Relay enabling circuits 2 NO instantaneous 2 NO delayed Us = 24 V DC screw terminal",311,"ΤΕΜ",1,"CP",1,"3SK11211CB41"]
["3SU1000-3AB61-0AK0","Twin pushbutton, 22 mm, round, plastic, white: I, Black: O, pushbuttons, flat",10.799999999999999,"ΤΕΜ",1,"CP",1,"3SU10003AB610AK0"]
["3SU1000-4GL11-0AA0","Key-operated switch O.M.R, 22 mm, round, plastic, lock number 73038, blue, with 2 keys, 3 switch positions I-O-II, latching, actuating angle 2x45Β°, 10:30h/12h/13:30h, Key removal I+O+II",38.4,"ΤΕΜ",1,"CP",1,"3SU10004GL110AA0"]
["3SU1001-0AB60-0AA0","Illuminated pushbutton, 22 mm, round, plastic, white, pushbutton, flat momentary contact type",6.63,"ΤΕΜ",1,"CP",1,"3SU10010AB600AA0"]
["3SU1002-2BL50-0AA0","Selector switch, illuminable, 22 mm, round, plastic, blue, selector switch, short, 3 switch positions I-O-II, latching, actuating angle 2x45Β°, 10:30h/12h/13:30h",10.4,"ΤΕΜ",1,"CP",1,"3SU10022BL500AA0"]
["3SU1030-1AA20-0AA0","Mushroom pushbutton, 22 mm, round, plastic with metal front ring, red, 30 mm, latching, Pull-to-unlatch mechanism",20.8,"ΤΕΜ",1,"CP",1,"3SU10301AA200AA0"]
["3SU1031-0AB00-0AA0","Illuminated pushbutton, 22 mm, round, plastic with metal front ring, amber, pushbutton, flat momentary contact type",7.42,"ΤΕΜ",1,"CP",1,"3SU10310AB000AA0"]
["3SU1032-2BN20-0AA0","Selector switch, illuminable, 22 mm, round, plastic with metal front ring, red, selector switch, short, 3 switch positions I-O<II, left latching, right momentary contact type, actuating angle 2x45Β°, 10:30h/12h/13:30h",11.6,"ΤΕΜ",1,"CP",1,"3SU10322BN200AA0"]
["3SU1050-1HA20-0AA0","EMERGENCY STOP mushroom pushbutton, 22 mm, round, metal, shiny, red, 40 mm, positive latching, acc. to EN ISO 13850, pull-to-unlatch mechanism",22.1,"ΤΕΜ",1,"CP",1,"3SU10501HA200AA0"]
["3SU1050-5HC01-0AA0","key-operated switch Siemens, 22 mm, round, metal, shiny, lock no. LSG1, with 2 keys, 2 switch positions O<I, momentary contact type, actuating angle 45Β°, 10:30h/12h, key removal O",65.099999999999994,"ΤΕΜ",1,"CP",1,"3SU10505HC010AA0"]
["3SU1050-5XM01-0AA0","Key-operated switch IKON, 22 mm, round, metal, shiny, lock number 360012K1, with 2 keys, 3 switch positions I>O<II, momentary contact type, actuating angle 2x45Β°, 10:30h/12h/13:30h, Key removal O",87.6,"ΤΕΜ",1,"CP",1,"3SU10505XM010AA0"]
["3SU1051-6AA70-0AA0","Indicator lights, 22 mm, round, metal, shiny, clear, lens, smooth",4.49,"ΤΕΜ",1,"CP",5,"3SU10516AA700AA0"]
["3SU1060-0JA10-0AA0","Pushbutton, 30 mm, round, metal, matte, black, front ring for flush installation, latching, Push-to-release mechanism",21.200000000000003,"ΤΕΜ",1,"CP",1,"3SU10600JA100AA0"]
["3SU1100-1HB20-1FJ0","EMERGENCY STOP mushroom pushbutton, 22 mm, round, plastic, red, 40 mm, positive latching, acc. to EN ISO 13850, rotate-to-unlatch, with yellow backing plate, inscription: ArrΓt d'urgence, with holder, 1 NO+1 NC, screw terminal",31.9,"ΤΕΜ",1,"CP",1,"3SU11001HB201FJ0"]
["3SU1102-0AB20-1FA0","Illuminated pushbutton, 22 mm, round, plastic, red, pushbutton, flat, momentary contact type, with holder, 1 NO+1 NC, LED module with integrated LED 24 V AC/DC, screw terminal",24.700000000000003,"ΤΕΜ",1,"CP",1,"3SU11020AB201FA0"]
["3SU1106-6AA20-3AA0","Indicator lights, 22 mm, round, plastic, red, lens, smooth, with holder, LED module, with integrated LED 230 V AC, Spring-type terminal",20.3,"ΤΕΜ",1,"CP",1,"3SU11066AA203AA0"]
["3SU1136-0AB20-1CA0","Illuminated pushbutton, 22 mm, round, plastic with metal front ring, red, pushbutton, flat, momentary contact type, with holder, 1 NC, LED module with integrated LED 230 V AC, screw terminal",27.700000000000003,"ΤΕΜ",1,"CP",1,"3SU11360AB201CA0"]
["3SU1150-0AB40-1FA0","Pushbutton, 22 mm, round, metal, shiny, green, pushbutton, flat, momentary contact type, 1 NO+1 NC, screw terminal",16.700000000000003,"ΤΕΜ",1,"CP",1,"3SU11500AB401FA0"]
["3SU1150-2CM60-1NA0","Toggle switch, 22 mm, round, metal, shiny, white, knob, long, 3 switch positions I>O<II, momentary contact type, actuating angle 2x45Β°, 10:30h/12h/13:30h, with holder, 1 NO, 1 NO, screw terminal",32.299999999999997,"ΤΕΜ",1,"CP",1,"3SU11502CM601NA0"]
["3SU1156-0AB00-1BA0","Illuminated pushbutton, 22 mm, round, metal, shiny, amber, pushbutton, flat, momentary contact type, with holder, 1 NO, LED module with integrated LED 230 V AC, screw terminal",28.200000000000003,"ΤΕΜ",1,"CP",1,"3SU11560AB001BA0"]
["3SU1400-1AA10-3QA0","Contact module with 2 contact elements, 1 NO+1 NC, gold-plated contacts, spring-type terminal, for front plate mounting",17.3,"ΤΕΜ",1,"CP",1,"3SU14001AA103QA0"]
["3SU1400-3AA10-5CA0","Contact module with 1 contact element, 1 NC, soldered connection, for use on printed circuit boards",5.89,"ΤΕΜ",1,"CP",1,"3SU14003AA105CA0"]
["3SU1401-1ME50-1DA1","SIRIUS ACT: terminal module (LED module), integrated LED blue, for front plate mounting, ATEX",37.6,"ΤΕΜ",1,"CP",1,"3SU14011ME501DA1"]
["3SU1501-1AG20-1FA0","holder, 3-way, plastic, 1 NO+1 NC, LED module, red, 6-24 V AC/DC, screw terminal",17.700000000000003,"ΤΕΜ",1,"CP",1,"3SU15011AG201FA0"]
["3SU1801-0AP00-4NB1","Enclosure for command devices 22 mm, round, enclosure material plastic, enclosure top part gray, 1 control point, plastic, A=Illuminated pushbutton yellow, momentary contact type, 40 mm, 1 NO, spring-type terminal,  LED module yellow, floor mounting, wired, recess for label, at bottom M12 connector 5-pole",84.199999999999989,"ΤΕΜ",1,"CP",1,"3SU18010AP004NB1"]
["3SU1851-0GB00-3BB1","Enclosure for command devices, 22 mm, round, enclosure material metal, enclosure top part gray, 1 control point metal, A=Mushroom pushbutton, black, 40 mm 1 NO, spring-type terminal, front mounting, label, silver, with inscription: Start, label glued in, 1xM20 each on top and bottom",65.8,"ΤΕΜ",1,"CP",1,"3SU18510GB003BB1"]
["3SU1900-0AC16-0AL0","Labeling plate for snapping on or gluing, on label holder, label size 12.5x27 mm, black label, white font, with inscription: Zu",99.5,"ΤΕΜ",100,"CP",10,"3SU19000AC160AL0"]
["3SU1900-0AC81-0AL0","Labeling plate for snapping on or gluing, on label holder, label size 12.5x27 mm, silver label, black font with inscription: Zu",99.5,"ΤΕΜ",100,"CP",10,"3SU19000AC810AL0"]
["3SU1900-0AC81-0QC0","Labeling plate for snapping on or gluing to label holder, label size 12.5x27mm, silver label, black font, with graphic symbol: II",99.5,"ΤΕΜ",100,"CP",10,"3SU19000AC810QC0"]
["3SU1900-0AE81-0AA0","Labeling plate for snapping on or gluing on label holder, Label size 27x27 mm, silver label, black font, without inscription, for self-labeling",90.1,"ΤΕΜ",100,"CP",10,"3SU19000AE810AA0"]
["3SU1900-0AF16-0QG0","Labeling plate for gluing on enclosure, label size 22x22 mm, black label, white font, with graphic symbol: O I",2.35,"ΤΕΜ",1,"CP",10,"3SU19000AF160QG0"]
["3SU1900-0DH70-0AA0","Silicone protection cap for Twin pushbutton, high, clear",3.91,"ΤΕΜ",1,"CP",1,"3SU19000DH700AA0"]
["3SU1950-0GA80-0AA0","USB port, 22 mm, metal shiny, silver",43.7,"ΤΕΜ",1,"CP",1,"3SU19500GA800AA0"]
["3SX3228","Separate actuator Universal radius actuator, for Position switch with separate actuator 3SE2243 and 3SE2257",11.9,"ΤΕΜ",1,"CP",1,"3SX3228"]
["3TC4417-0CM4","Contactor size 2, 2-pole DC-3 and 5, 32 A Auxiliary switch 22 (2 NO + 2 NC) DC operation 220 V DC",516,"ΤΕΜ",1,"CP",1,"3TC44170CM4"]
["3TC5217-5KB4","Contactor size 8, 2-pole DC-4, Rated operating current 220 A Auxiliary switch 22 (2 NO + 2 NC) Direct current operation G drive with integrated varistor 24 V DC",1851,"ΤΕΜ",1,"CP",1,"3TC52175KB4"]
["3TD2002-2QM6","Contactor assembly for reversing Size 00, AC-3, 4 kW/400 V Alternating current operation 220 V AC 60 Hz 200 V AC 50 Hz !!! Phased-out product !!! Successor is SIRIUS 3RA23",226,"ΤΕΜ",1,"CP",1,"3TD20022QM6"]
["3TF2010-0AF0","Contactor, Size 00, 3-pole, AC-3 4 kW/400 V; Screw terminal Auxiliary switch 10E (1 NO) 110 V AC 50 Hz/132 V AC 60 Hz AC operation !!! Phased-out product !!! Successor is SIRIUS 3RT201 or 3TG10",57.9,"ΤΕΜ",1,"CP",1,"3TF20100AF0"]
["3TF2222-0AC2","Contactor, Size 00, 3-pole, AC-3 4 kW/400 V; Screw terminal Auxiliary switch 22E (2 NO + 2 NC) Width 45 mm 24 V AC 50/60 Hz AC operation !!! Phased-out product !!! Successor is SIRIUS 3RT201 or 3TG10",77.199999999999989,"ΤΕΜ",1,"CP",1,"3TF22220AC2"]
["3TH2022-0BF4","Contactor relay, 22E, EN 50011, 2 NO + 2 NC, Screw terminal DC operation 110 V DC !!! Phased-out product !!! Successor is SIRIUS 3RH21",68.3,"ΤΕΜ",1,"CP",1,"3TH20220BF4"]
["3TH2031-0AG1","Contactor relay, 31E, EN 50011, 3 NO + 1 NC, Screw terminal AC operation 110 V 60 Hz/92 V AC 50 Hz !!! Phased-out product !!! Successor is SIRIUS 3RH21",62.6,"ΤΕΜ",1,"CP",1,"3TH20310AG1"]
["3TH2040-0AF0","Contactor relay, 40E, EN 50011, 4 NO; Screw terminal AC operation 110 V AC 50 Hz/132 V AC 60 Hz !!! Phased-out product !!! Successor is SIRIUS 3RH21",60,"ΤΕΜ",1,"CP",1,"3TH20400AF0"]
["3TH2244-1BB4","Contactor relay, 44E, EN 50011, 4 NO + 4 NC flat connector terminal Width 45 mm 24 V DC DC operation !!! Phased-out product !!! Successor is SIRIUS 3RH21",112,"ΤΕΜ",1,"CP",1,"3TH22441BB4"]
["3TH4244-0AP2","Contactor relay, 44E, DIN EN 50011, 4NO + 4NC, screw terminal AC operation 240 V AC 50/60 Hz",74.399999999999991,"ΤΕΜ",1,"CP",1,"3TH42440AP2"]
["3TH4253-0AK6","Contactor relay, 53E, DIN EN 50011, 5NO + 3NC, screw terminal AC operation 120 V AC 60 Hz/110 V AC 50 Hz",71.5,"ΤΕΜ",1,"CP",1,"3TH42530AK6"]
["3TH4271-0AL2","Contactor relay, 71E, DIN EN 50011, 7 NO + 1 NC, screw terminal AC operation 230 V AC 50/60 Hz",71.5,"ΤΕΜ",1,"CP",1,"3TH42710AL2"]
["3TH4364-0AU0","Contactor relay, 64E, EN 50011, 6NO + 4NC, screw terminal, AC operation, 240 V AC 50 Hz/288 V AC 60 Hz",114,"ΤΕΜ",1,"CP",1,"3TH43640AU0"]
["3TH4373-0BE4","Contactor relay, 73E, EN 50011, 7 NO + 3 NC, screw terminal, DC operation, 60 V DC",164,"ΤΕΜ",1,"CP",1,"3TH43730BE4"]
["3TK1974-0AU0","Coil for 3TK14, 3TK15, 3TK17, 230...240 V AC, 50 Hz",310,"ΤΕΜ",1,"CP",1,"3TK19740AU0"]
["3TK2040-4AV0","Miniature contactor, Screw terminal, 4 NO Screw mounting (diagonal) 400/380 V AC 50 Hz, 480/460 V 60 Hz AC operation !!! Phased-out product !!! Successor is SIRIUS 3RT23/25",64,"ΤΕΜ",1,"CP",1,"3TK20404AV0"]
["3TX4490-4H","Surge suppressor Varistor with LED 48...127 V AC/24...70 V DC for plugging onto contactors without/with auxiliary switch blocks",15,"ΤΕΜ",1,"CP",1,"3TX44904H"]
["3TX7014-7BP00","Relay, 1 changeover contact, 60 V DC, can be used with 115/230 V AC/DC complete unit",13.2,"ΤΕΜ",1,"CP",20,"3TX70147BP00"]
["3TY2781-2C","Auxiliary switch block, 2 NO+2 NC, left",69.199999999999989,"ΤΕΜ",1,"CP",1,"3TY27812C"]
["3TY5892-0BE4","Closing latching for contactor 3TL8 operating voltage DC 60V",1024,"ΤΕΜ",1,"LP",1,"3TY58920BE4"]
["3TY6483-0BY80-0AC1","Magnet coil 254-281 ohm 2x 4986 WD 70 V DC",174,"ΤΕΜ",1,"CP",1,"3TY64830BY800AC1"]
["3TY6523-0AR1","Magnet coil for 3TC52 440 V AC 60 Hz/367 V AC 50 Hz",154,"ΤΕΜ",1,"CP",1,"3TY65230AR1"]
["3TY7463-0AJ2","Magnet coil for Contactors 3TF46/47 115 V AC 50/60 Hz",78,"ΤΕΜ",1,"CP",1,"3TY74630AJ2"]
["3TY7563-0AP6","Magnet coil for contactors 3TF56 and 3TK56 240 V AC 60 Hz/220 V AC 50 Hz",142,"ΤΕΜ",1,"CP",1,"3TY75630AP6"]
["3UF1900-0K","Motherboard for stand-alone installation for converter 3UF18 47, 3UF18 48",31.6,"ΤΕΜ",1,"CP",1,"3UF19000K"]
["3UG4511-2AN20","Analog monitoring relay Phase sequence monitoring 3 x 160...260 V 50...60 Hz AC 1 change-over contact spring-type connection system",86.8,"ΤΕΜ",1,"CP",1,"3UG45112AN20"]
["3VA1010-2ED32-0JC0","Circuit breaker 3VA1 IEC Frame 100 Switching capacity class B Icu=16 kA @ 415 V 3-pole, system protection TM210, FTFM, In=100 A Overload protection Ir=100 A non-adjustable short-circuit protection Ii = 10 x In Lug terminal Shunt release (STL) 110-127 V DC, 50/60 Hz AC 2 auxiliary switches HQ",242.59,"ΤΕΜ",1,"LP",1,"3VA10102ED320JC0"]
["3VA1010-3ED36-0HA0","Circuit breaker 3VA1 IEC Frame 100 Switching capacity class N Icu=25 kA @ 415 V 3-pole, system protection TM210, FTFM, In=100 A Overload protection Ir=100 A non-adjustable short-circuit protection Ii = 10 x In Terminal connection Shunt release (STL) 12-30 V DC, 24 V AC 50/60 Hz",229.04999999999998,"ΤΕΜ",1,"LP",1,"3VA10103ED360HA0"]
["3VA1010-4ED36-0CC0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=100A overload protection Ir=100A fixed short-circuit protection Ii=10 x In clamp connection undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ",288.38,"ΤΕΜ",1,"LP",1,"3VA10104ED360CC0"]
["3VA1020-2ED32-0AE0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 3-pole, line protection TM210, FTFM, In=20A overload protection Ir=20A fixed short-circuit protection Ii=16 x In nut keeper kit 4 auxiliary switches HQ",197.57,"ΤΕΜ",1,"LP",1,"3VA10202ED320AE0"]
["3VA1020-4ED36-0BH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=20A overload protection Ir=20A fixed short-circuit protection Ii=16 x In clamp connection undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ",279.89,"ΤΕΜ",1,"LP",1,"3VA10204ED360BH0"]
["3VA1025-4ED32-0HA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=25A overload protection Ir=25A fixed short-circuit protection Ii=12.8 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz",196.39999999999998,"ΤΕΜ",1,"LP",1,"3VA10254ED320HA0"]
["3VA1032-2ED32-0KH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 3-pole, line protection TM210, FTFM, In=32A overload protection Ir=32A fixed short-circuit protection Ii=10 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ",241.08,"ΤΕΜ",1,"LP",1,"3VA10322ED320KH0"]
["3VA1032-4ED36-0AA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=32A overload protection Ir=32A fixed short-circuit protection Ii=10 x In clamp connection",152.29999999999998,"ΤΕΜ",1,"LP",1,"3VA10324ED360AA0"]
["3VA1040-3ED32-0HH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM210, FTFM, In=40A overload protection Ir=40A fixed short-circuit protection Ii=10 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",243.44,"ΤΕΜ",1,"LP",1,"3VA10403ED320HH0"]
["3VA1050-2ED32-0CC0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 3-pole, line protection TM210, FTFM, In=50A overload protection Ir=50A fixed short-circuit protection Ii=10 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ",241.67,"ΤΕΜ",1,"LP",1,"3VA10502ED320CC0"]
["3VA1050-3ED32-0AD0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM210, FTFM, In=50A overload protection Ir=50A fixed short-circuit protection Ii=10 x In nut keeper kit 3 auxiliary switches HQ",184.64,"ΤΕΜ",1,"LP",1,"3VA10503ED320AD0"]
["3VA1050-4ED42-0JH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM210, FTFM, In=50A overload protection Ir=50A fixed short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",288.12,"ΤΕΜ",1,"LP",1,"3VA10504ED420JH0"]
["3VA1063-3ED32-0AC0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM210, FTFM, In=63A overload protection Ir=63A fixed short-circuit protection Ii=10 x In nut keeper kit 2 auxiliary switches HQ",167,"ΤΕΜ",1,"LP",1,"3VA10633ED320AC0"]
["3VA1063-4ED32-0JH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=63A overload protection Ir=63A fixed short-circuit protection Ii=10 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",245.79,"ΤΕΜ",1,"LP",1,"3VA10634ED320JH0"]
["3VA1063-4ED36-0HH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=63A overload protection Ir=63A fixed short-circuit protection Ii=10 x In clamp connection shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",262.25,"ΤΕΜ",1,"LP",1,"3VA10634ED360HH0"]
["3VA1080-2ED42-0DC0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 4-pole, line protection TM210, FTFM, In=80A overload protection Ir=80A fixed short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",296.94,"ΤΕΜ",1,"LP",1,"3VA10802ED420DC0"]
["3VA1080-3ED42-0JH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 4-pole, line protection TM210, FTFM, In=80A overload protection Ir=80A fixed short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",299.88,"ΤΕΜ",1,"LP",1,"3VA10803ED420JH0"]
["3VA1080-4ED42-0AE0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM210, FTFM, In=80A overload protection Ir=80A fixed short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit 4 auxiliary switches HQ",261.66000000000003,"ΤΕΜ",1,"LP",1,"3VA10804ED420AE0"]
["3VA1110-1AA32-0AA0","switch disconnector 3VA1 IEC frame 160 3-pole SD100, In=100A without overload protection w/o short-circuit protection nut keeper kit",154.64999999999998,"ΤΕΜ",1,"LP",1,"3VA11101AA320AA0"]
["3VA1110-3EF32-0CC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ",268.86,"ΤΕΜ",1,"LP",1,"3VA11103EF320CC0"]
["3VA1110-4EE32-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM220, ATFM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=10 x In nut keeper kit",147.98999999999998,"ΤΕΜ",1,"LP",1,"3VA11104EE320AA0"]
["3VA1110-5ED32-0KA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM210, FTFM, In=100A overload protection Ir=100A fixed short-circuit protection Ii=10 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC",271.65999999999997,"ΤΕΜ",1,"LP",1,"3VA11105ED320KA0"]
["3VA1110-5EE36-0BF0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM220, ATFM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=10 x In clamp connection circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM220, ATFM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=10 x In clamp UNDERVOLTAGE RELEASE 24 V DC ACCESSORY FOR 3VA1 and 3VA20 up 1 AUXILIARY SWITCH CHANGEOVER H 1 TRIP ALARM SWITCH CHANGEOVER",343.4,"ΤΕΜ",1,"LP",1,"3VA11105EE360BF0"]
["3VA1110-5EF36-0KC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=5...10 x In clamp connection shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ",336.34,"ΤΕΜ",1,"LP",1,"3VA11105EF360KC0"]
["3VA1110-6EF32-0AE0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=5...10 x In nut keeper kit 4 auxiliary switches HQ",315.76,"ΤΕΜ",1,"LP",1,"3VA11106EF320AE0"]
["3VA1110-6MH32-0KH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, starter protection TM120M, AM, In=100A without overload protection short-circuit protection Ii=5...15 x In nut keeper kit shunt trip (STL) 220-250 V DC; 208-277 V AC 2 auxiliary switches HQ 1 trip alarm switch HQ",358.09999999999997,"ΤΕΜ",1,"LP",1,"3VA11106MH320KH0"]
["3VA1112-1AA42-0JC0","switch disconnector 3VA1 IEC frame 160 4-pole SD100, In=125A without overload protection w/o short-circuit protection nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",354.57,"ΤΕΜ",1,"LP",1,"3VA11121AA420JC0"]
["3VA1112-4EE42-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM220, ATFM, In=125A overload protection Ir=88A...125A short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit",240.17,"ΤΕΜ",1,"LP",1,"3VA11124EE420AA0"]
["3VA1112-5ED32-0AD0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM210, FTFM, In=125A overload protection Ir=125A fixed short-circuit protection Ii=10 x In nut keeper kit 3 auxiliary switches HQ",391.02,"ΤΕΜ",1,"LP",1,"3VA11125ED320AD0"]
["3VA1112-5EF36-0AB0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=125A overload protection Ir=88A...125A short-circuit protection Ii=5...10 x In clamp connection 2 auxiliary switches HP",403.4,"ΤΕΜ",1,"LP",1,"3VA11125EF360AB0"]
["3VA1112-6EF32-0BA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=125A overload protection Ir=88A...125A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 24V DC",394.17,"ΤΕΜ",1,"LP",1,"3VA11126EF320BA0"]
["3VA1112-6MH36-0KA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, starter protection TM120M, AM, In=125A without overload protection short-circuit protection Ii=5...15 x In clamp connection shunt trip (STL) 220-250 V DC; 208-277 V AC",476.28,"ΤΕΜ",1,"LP",1,"3VA11126MH360KA0"]
["3VA1116-1AA32-0CH0","switch disconnector 3VA1 IEC frame 160 3-pole SD100, In=160A without overload protection w/o short-circuit protection nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",342.21999999999997,"ΤΕΜ",1,"LP",1,"3VA11161AA320CH0"]
["3VA1116-3ED12-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 240V 1-pole, line protection TM210, FTFM, In=160A overload protection Ir=160A fixed short-circuit protection Ii=10 x In nut keeper kit",144.57,"ΤΕΜ",1,"LP",1,"3VA11163ED120AA0"]
["3VA1116-4EF32-0JA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz",355.27,"ΤΕΜ",1,"LP",1,"3VA11164EF320JA0"]
["3VA1116-5ED46-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM210, FTFM, In=160A overload protection Ir=160A fixed short-circuit protection Ii=10 x In N conductor unprotected clamp connection",482.64,"ΤΕΜ",1,"LP",1,"3VA11165ED460AA0"]
["3VA1116-5EF32-0HA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz",403.68,"ΤΕΜ",1,"LP",1,"3VA11165EF320HA0"]
["3VA1116-6EF36-0AB0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In clamp connection 2 auxiliary switches HP",439.62,"ΤΕΜ",1,"LP",1,"3VA11166EF360AB0"]
["3VA1120-3EF32-0DH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=20A overload protection Ir=14A...20A short-circuit protection Ii=8...16 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",276.95,"ΤΕΜ",1,"LP",1,"3VA11203EF320DH0"]
["3VA1120-4EF36-0HA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=20A overload protection Ir=14A...20A short-circuit protection Ii=8...16 x In clamp connection shunt trip (STL) 12-30V DC, 24V AC 50/60Hz",239.32,"ΤΕΜ",1,"LP",1,"3VA11204EF360HA0"]
["3VA1120-5ED46-0AB0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM210, FTFM, In=20A overload protection Ir=20A fixed short-circuit protection Ii=16 x In N conductor unprotected clamp connection circuit breaker 3VA1 IEC frame 160 2 auxiliary switches HP",244.48999999999998,"ΤΕΜ",1,"LP",1,"3VA11205ED460AB0"]
["3VA1120-6EF36-0CA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=20A overload protection Ir=14A...20A short-circuit protection Ii=8...16 x In clamp connection undervoltage release (UVR) 120-127V AC 50/60Hz",288.70999999999998,"ΤΕΜ",1,"LP",1,"3VA11206EF360CA0"]
["3VA1125-3EF32-0KA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=25A overload protection Ir=18A...25A short-circuit protection Ii=6.4...12.8 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC",209.92,"ΤΕΜ",1,"LP",1,"3VA11253EF320KA0"]
["3VA1125-5EF32-0AC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=25A overload protection Ir=18A...25A short-circuit protection Ii=6.4...12.8 x In nut keeper kit 2 auxiliary switches HQ",213.45,"ΤΕΜ",1,"LP",1,"3VA11255EF320AC0"]
["3VA1125-6GD42-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 4-pole, line protection TM210, FTFM, In=25A overload protection Ir=25A fixed short-circuit protection Ii=12.8 x In N conductor protection 100% nut keeper kit",236.97,"ΤΕΜ",1,"LP",1,"3VA11256GD420AA0"]
["3VA1132-4EF32-0BA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=32A overload protection Ir=22A...32A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 24V DC",240.5,"ΤΕΜ",1,"LP",1,"3VA11324EF320BA0"]
["3VA1132-5EF32-0KC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=32A overload protection Ir=22A...32A short-circuit protection Ii=5...10 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ",272.25,"ΤΕΜ",1,"LP",1,"3VA11325EF320KC0"]
["3VA1132-6EF36-0AM0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=32A overload protection Ir=22A...32A short-circuit protection Ii=5...10 x In clamp connection 2 auxiliary switches 1 short circuit alarm switch",269.89999999999998,"ΤΕΜ",1,"LP",1,"3VA11326EF360AM0"]
["3VA1140-3EF32-0DH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=40A overload protection Ir=28A...40A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",276.95,"ΤΕΜ",1,"LP",1,"3VA11403EF320DH0"]
["3VA1140-4GF42-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM240, ATAM, In=40A overload protection Ir=28A...40A short-circuit protection Ii=5...10 x In N conductor protection 100% nut keeper kit",212.85999999999999,"ΤΕΜ",1,"LP",1,"3VA11404GF420AA0"]
["3VA1140-5EF32-0AE0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=40A overload protection Ir=28A...40A short-circuit protection Ii=5...10 x In nut keeper kit 4 auxiliary switches HQ",245.79,"ΤΕΜ",1,"LP",1,"3VA11405EF320AE0"]
["3VA1150-3EF32-0BC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=50A overload protection Ir=35A...50A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ",261.08,"ΤΕΜ",1,"LP",1,"3VA11503EF320BC0"]
["3VA1150-3EF36-0AE0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=50A overload protection Ir=35A...50A short-circuit protection Ii=5...10 x In clamp connection 4 auxiliary switches HQ",232.85,"ΤΕΜ",1,"LP",1,"3VA11503EF360AE0"]
["3VA1150-5EF32-0AB0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=50A overload protection Ir=35A...50A short-circuit protection Ii=5...10 x In nut keeper kit 2 auxiliary switches HP",228.73999999999998,"ΤΕΜ",1,"LP",1,"3VA11505EF320AB0"]
["3VA1150-5GE46-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM220, ATFM, In=50A overload protection Ir=35A...50A short-circuit protection Ii=10 x In N conductor protection 100% clamp connection",242.26,"ΤΕΜ",1,"LP",1,"3VA11505GE460AA0"]
["3VA1163-1AA32-0AF0","switch disconnector 3VA1 IEC frame 160 3-pole SD100, In=63A without overload protection w/o short-circuit protection nut keeper kit 1 auxiliary switch HQ 1 trip alarm switch HQ",155.23999999999998,"ΤΕΜ",1,"LP",1,"3VA11631AA320AF0"]
["3VA1163-3EF32-0AE0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=63A overload protection Ir=44A...63A short-circuit protection Ii=5...10 x In nut keeper kit 4 auxiliary switches HQ",216.98,"ΤΕΜ",1,"LP",1,"3VA11633EF320AE0"]
["3VA1163-4EF36-0AH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=63A overload protection Ir=44A...63A short-circuit protection Ii=5...10 x In clamp connection 2 auxiliary switches HQ 1 trip alarm switch HQ",228.14999999999998,"ΤΕΜ",1,"LP",1,"3VA11634EF360AH0"]
["3VA1163-5EF32-0AD0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=63A overload protection Ir=44A...63A short-circuit protection Ii=5...10 x In nut keeper kit 3 auxiliary switches HQ",228.73999999999998,"ΤΕΜ",1,"LP",1,"3VA11635EF320AD0"]
["3VA1163-5MH32-0HH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, starter protection TM120M, AM, In=63A without overload protection short-circuit protection Ii=5...15 x In nut keeper kit shunt trip (STL) 12-30 V DC; 24 V AC 50/60 Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",289.89,"ΤΕΜ",1,"LP",1,"3VA11635MH320HH0"]
["3VA1163-6EF32-0HC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=63A overload protection Ir=44A...63A short-circuit protection Ii=5...10 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ",288.70999999999998,"ΤΕΜ",1,"LP",1,"3VA11636EF320HC0"]
["3VA1163-6MH32-0JH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, starter protection TM120M, AM, In=63A without overload protection short-circuit protection Ii=5...15 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",305.76,"ΤΕΜ",1,"LP",1,"3VA11636MH320JH0"]
["3VA1180-3EF32-0KC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=80A overload protection Ir=56A...80A short-circuit protection Ii=5...10 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ",231.32999999999998,"ΤΕΜ",1,"LP",1,"3VA11803EF320KC0"]
["3VA1180-4EF36-0KH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=80A overload protection Ir=56A...80A short-circuit protection Ii=5...10 x In clamp connection shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ",304.58999999999997,"ΤΕΜ",1,"LP",1,"3VA11804EF360KH0"]
["3VA1180-5EF36-0JC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=80A overload protection Ir=56A...80A short-circuit protection Ii=5...10 x In clamp connection shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",305.76,"ΤΕΜ",1,"LP",1,"3VA11805EF360JC0"]
["3VA1196-3EF32-0AH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=16A overload protection Ir=11A...16A short-circuit protection Ii=10...20 x In nut keeper kit 2 auxiliary switches HQ 1 trip alarm switch HQ",199.92,"ΤΕΜ",1,"LP",1,"3VA11963EF320AH0"]
["3VA1196-4EF36-0JC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=16A overload protection Ir=11A...16A short-circuit protection Ii=10...20 x In clamp connection shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",271.65999999999997,"ΤΕΜ",1,"LP",1,"3VA11964EF360JC0"]
["3VA1196-5EF32-0KC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=16A overload protection Ir=11A...16A short-circuit protection Ii=10...20 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ",272.25,"ΤΕΜ",1,"LP",1,"3VA11965EF320KC0"]
["3VA1216-5EF32-0BC0","circuit breaker 3VA1 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 24V DC",522.52,"ΤΕΜ",1,"LP",1,"3VA12165EF320BC0"]
["3VA1216-5MH32-0AA0","circuit breaker 3VA1 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, starter protection TM120M, AM, In=160A without overload protection short-circuit protection Ii=7...16 x In nut keeper kit",429.24,"ΤΕΜ",1,"LP",1,"3VA12165MH320AA0"]
["3VA1220-5EF32-0JC0","circuit breaker 3VA1 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=200A overload protection Ir=140A...200A short-circuit protection Ii=5...10 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",522.52,"ΤΕΜ",1,"LP",1,"3VA12205EF320JC0"]
["3VA1220-5EF42-0HG0","Circuit breaker 3VA1 IEC Frame 250 Switching capacity class M Icu=55 kA @ 415 V 4-pole, system protection TM240, ATAM, In=200 A Overload protection Ir=140 A...200 A short-circuit protection Ii=5...10 x In N-conductor unprotected Lug terminal Circuit breaker 3VA1 IEC Frame 250 Shunt release left 24 V AC 50/60 Hz/24-30 V DC 1 auxiliary switch HP 1 tripped signaling contact HP",697.95,"ΤΕΜ",1,"LP",1,"3VA12205EF420HG0"]
["3VA1220-6EF42-0DH0","circuit breaker 3VA1 IEC frame 250 breaking capacity class H Icu=70kA @ 415V 4-pole, line protection TM240, ATAM, In=200A overload protection Ir=140A...200A short-circuit protection Ii=5...10 x In N conductor unprotected nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",659.81999999999994,"ΤΕΜ",1,"LP",1,"3VA12206EF420DH0"]
["3VA1225-1AA32-0HC0","switch disconnector 3VA1 IEC frame 250 3-pole SD100, In=250A without overload protection w/o short-circuit protection nut keeper kit shunt trip (STL) 12-30V DC; 24 V AC 50/60 Hz 2 auxiliary switches HQ",451,"ΤΕΜ",1,"LP",1,"3VA12251AA320HC0"]
["3VA1225-4EF42-0AF0","circuit breaker 3VA1 IEC frame 250 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM240, ATAM, In=250A overload protection Ir=175A...250A short-circuit protection Ii=5...10 x In N conductor unprotected nut keeper kit 1 auxiliary switch HQ 1 trip alarm switch HQ",538.63,"ΤΕΜ",1,"LP",1,"3VA12254EF420AF0"]
["3VA1225-5EF42-0CC0","circuit breaker 3VA1 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM240, ATAM, In=250A overload protection Ir=175A...250A short-circuit protection Ii=5...10 x In N conductor unprotected nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz",638.81999999999994,"ΤΕΜ",1,"LP",1,"3VA12255EF420CC0"]
["3VA1225-6EF42-0AF0","circuit breaker 3VA1 IEC frame 250 breaking capacity class H Icu=70kA @ 415V 4-pole, line protection TM240, ATAM, In=250A overload protection Ir=175A...250A short-circuit protection Ii=5...10 x In N conductor unprotected nut keeper kit 1 auxiliary switch HQ 1 trip alarm switch HQ",561.30999999999995,"ΤΕΜ",1,"LP",1,"3VA12256EF420AF0"]
["3VA1332-6MH32-0AC0","circuit breaker 3VA1 IEC frame 400 breaking capacity class H Icu=70kA @ 415V 3-pole, starter protection TM120M, AM, In=320A without overload protection short-circuit protection Ii=8...16 x In nut keeper kit circuit breaker 3VA1 IEC frame 400 breaking capacity class H Icu=70kA @ 415V 3-pole, starter protection TM120M, AM, In=320A without overload protection short-circuit protection Ii=8...16 x In nut keeper kit 2 AUXILIARY SWITCH CHANGEOVER H",976.08,"ΤΕΜ",1,"LP",1,"3VA13326MH320AC0"]
["3VA1450-5MH32-0AA0","circuit breaker 3VA1 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 3-pole, starter protection TM120M, AM, In=500A without overload protection short-circuit protection Ii=8...16 x In nut keeper kit",940.28,"ΤΕΜ",1,"LP",1,"3VA14505MH320AA0"]
["3VA1463-7EF32-0AJ0","circuit breaker 3VA1 IEC frame 630 breaking capacity class C Icu=110kA @ 415 V 3-pole, line protection TM240, ATAM, In=630A overload protection Ir=440A ...630A short-circuit protection Ii=4...8 x In nut keeper kit circuit breaker 3VA1 IEC frame 630 breaking capacity class C Icu=110kA @ 415 V 3-pole, line protection TM240, ATAM, In=630A overload protection Ir=440A ...630A short-circuit protection Ii=4...8 x In nut 2 AUXILIARY SWITCH CHANGEOVER H 1 TRIP ALARM SWITCH CHANGEOVER",2193.2399999999998,"ΤΕΜ",1,"LP",1,"3VA14637EF320AJ0"]
["3VA1563-7MH32-0AA0","circuit breaker 3VA1 IEC frame 1000 breaking capacity class C Icu=110kA @ 415V 3-pole, starter protection TM120M, AM, In=630A without overload protection short-circuit protection Ii=8...15 x In nut keeper kit",1245.32,"ΤΕΜ",1,"LP",1,"3VA15637MH320AA0"]
["3VA2010-5HN32-0AH0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit 2 auxiliary switches HQ 1 trip alarm switch HQ",433.36,"ΤΕΜ",1,"LP",1,"3VA20105HN320AH0"]
["3VA2010-5JP36-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU550, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% clamp connection",606.16,"ΤΕΜ",1,"LP",1,"3VA20105JP360AA0"]
["3VA2010-6HL32-0JC0","circuit breaker 3VA2 IEC frame 100 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU320, LI, In=100A overload protection Ir=40A...100A short-circuit protection Ii=1.5...12 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",475.52,"ΤΕΜ",1,"LP",1,"3VA20106HL320JC0"]
["3VA2010-7HN36-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In clamp connection",468.53,"ΤΕΜ",1,"LP",1,"3VA20107HN360AA0"]
["3VA2025-5HM46-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU330, LIG, In=25A overload protection Ir=10A...25A short-circuit protection Ii=1.5...12 x In N conductor protection adjustable (OFF, 100%) ground-fault protection Ig=0.6...1 x In= tg=0.1/0.3s clamp connection",597.05999999999995,"ΤΕΜ",1,"LP",1,"3VA20255HM460AA0"]
["3VA2025-7KQ42-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class C Icu=110kA @ 415V 4-pole, line protection ETU860, LSIG, In=25A overload protection Ir=10A...25A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) gr.-fault prot., can be sw. off Ig=0.2...1 x In= tg=0.05-0.8s nut keeper kit",923.23,"ΤΕΜ",1,"LP",1,"3VA20257KQ420AA0"]
["3VA2040-5JP32-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU550, LSI, In=40A overload protection Ir=16A...40A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit",571.16999999999996,"ΤΕΜ",1,"LP",1,"3VA20405JP320AA0"]
["3VA2063-5HL36-0BL0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=63A overload protection Ir=25A...63A short-circuit protection Ii=1.5...12 x In clamp connection undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",482.51,"ΤΕΜ",1,"LP",1,"3VA20635HL360BL0"]
["3VA2063-5HL36-0HA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=63A overload protection Ir=25A...63A short-circuit protection Ii=1.5...12 x In clamp connection shunt trip (STL) 12-30V DC, 24V AC 50/60Hz",393.21999999999997,"ΤΕΜ",1,"LP",1,"3VA20635HL360HA0"]
["3VA2063-5JQ32-0DH0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU560, LSIG, In=63A overload protection Ir=25A...63A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer gr.-fault prot., can be sw. off Ig=0.25...1 x In, tg=0.05-0.8s nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",823.21,"ΤΕΜ",1,"LP",1,"3VA20635JQ320DH0"]
["3VA2063-6HN32-0AJ0","circuit breaker 3VA2 IEC frame 100 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit 2 auxiliary switches HP 1 trip alarm switch HP",468.51,"ΤΕΜ",1,"LP",1,"3VA20636HN320AJ0"]
["3VA2063-7KP36-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU850, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% clamp connection",767.18999999999994,"ΤΕΜ",1,"LP",1,"3VA20637KP360AA0"]
["3VA2110-5HL32-0AC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=100A overload protection Ir=40A...100A short-circuit protection Ii=1.5...12 x In nut keeper kit 2 auxiliary switches HQ",377.69,"ΤΕΜ",1,"LP",1,"3VA21105HL320AC0"]
["3VA2110-5HN36-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In clamp connection",401.8,"ΤΕΜ",1,"LP",1,"3VA21105HN360AA0"]
["3VA2110-5HN36-0HA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In clamp connection shunt trip (STL) 12-30V DC, 24V AC 50/60Hz",458.93,"ΤΕΜ",1,"LP",1,"3VA21105HN360HA0"]
["3VA2110-5JQ32-0KC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU560, LSIG, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit shunt trip (STL) 220-250V DC; 208-277V AC 2 auxiliary switches HQ",808.21,"ΤΕΜ",1,"LP",1,"3VA21105JQ320KC0"]
["3VA2110-5MN36-0BL0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=3...15 x Ir, Ii=15 x In clamp connection undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",530.21,"ΤΕΜ",1,"LP",1,"3VA21105MN360BL0"]
["3VA2110-6HN36-0HA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In clamp connection shunt trip (STL) 12-30V DC, 24V AC 50/60Hz",498.07,"ΤΕΜ",1,"LP",1,"3VA21106HN360HA0"]
["3VA2110-7HN42-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 4-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In N conductor protection adjustable (OFF, 50%, 100%) nut keeper kit",567.77,"ΤΕΜ",1,"LP",1,"3VA21107HN420AA0"]
["3VA2110-7MS32-0BH0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 3-pole, starter protection ETU310M, I, In=100A overload protection Ir=40A...100A short-circuit protection Ii=3...15 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ",430.38,"ΤΕΜ",1,"LP",1,"3VA21107MS320BH0"]
["3VA2110-8HL36-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class L Icu=150kA @ 415V 3-pole, line protection ETU320, LI, In=100A overload protection Ir=40A...100A short-circuit protection Ii=1.5...12 x In clamp connection",481.53,"ΤΕΜ",1,"LP",1,"3VA21108HL360AA0"]
["3VA2116-5HL36-0KL0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=160A overload protection Ir=63A...160A short-circuit protection Ii=1.5...10 x In clamp connection shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",671.06999999999994,"ΤΕΜ",1,"LP",1,"3VA21165HL360KL0"]
["3VA2116-5JQ32-0CH0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU560, LSIG, In=160A overload protection Ir=63A...160A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",994.24,"ΤΕΜ",1,"LP",1,"3VA21165JQ320CH0"]
["3VA2116-6HL32-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU320, LI, In=160A overload protection Ir=63A...160A short-circuit protection Ii=1.5...10 x In nut keeper kit",585.04,"ΤΕΜ",1,"LP",1,"3VA21166HL320AA0"]
["3VA2116-6HN32-0JL0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=160A overload protection Ir=63A...160A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",749.03,"ΤΕΜ",1,"LP",1,"3VA21166HN320JL0"]
["3VA2125-0HM46-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class  E Icu=200 kA @ 415 V 4-pole, line protection ETU330,  LIG, In=25A overload protection Ir=10A ... 25A short circuit protection Ii=1,5...12 x In neutral protection adjustable(OFF 100%) ground fault protection Ig=0,6... 1 x In, tg=0,1/0,3s cable connection",823.62,"ΤΕΜ",1,"LP",1,"3VA21250HM460AA0"]
["3VA2125-5HK42-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU340, ELISA LI, In=25A overload protection Ir=10A...25A short-circuit protection Ii=15 x In N conductor protection adjustable (OFF, 100%) nut keeper kit",404.81,"ΤΕΜ",1,"LP",1,"3VA21255HK420AA0"]
["3VA2125-7HN42-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 4-pole, line protection ETU350, LSI, In=25A overload protection Ir=10A...25A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In N conductor protection adjustable (OFF, 100%) nut keeper kit",525.66,"ΤΕΜ",1,"LP",1,"3VA21257HN420AA0"]
["3VA2140-5HK32-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU340, ELISA LI, In=40A overload protection Ir=16A...40A short-circuit protection Ii=15 x In nut keeper kit",319.52999999999997,"ΤΕΜ",1,"LP",1,"3VA21405HK320AA0"]
["3VA2140-7KP42-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 4-pole, line protection ETU850, LSI, In=40A overload protection Ir=16A...40A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) nut keeper kit",838.2,"ΤΕΜ",1,"LP",1,"3VA21407KP420AA0"]
["3VA2140-8JQ36-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class L Icu=150kA @ 415V 3-pole, line protection ETU560, LSIG, In=40A overload protection Ir=16A...40A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.4... 1 x In, tg=0.05-0.8s clamp connection",833.2,"ΤΕΜ",1,"LP",1,"3VA21408JQ360AA0"]
["3VA2163-5HL36-0JC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=63A overload protection Ir=25A...63A short-circuit protection Ii=1.5...12 x In clamp connection shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",426.37,"ΤΕΜ",1,"LP",1,"3VA21635HL360JC0"]
["3VA2163-5HN36-0DH0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In clamp connection undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",499.08,"ΤΕΜ",1,"LP",1,"3VA21635HN360DH0"]
["3VA2163-5KP32-0DL0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU850, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",823.21,"ΤΕΜ",1,"LP",1,"3VA21635KP320DL0"]
["3VA2163-5MN32-0BA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit undervoltage release (UVR) 24V DC",425.36,"ΤΕΜ",1,"LP",1,"3VA21635MN320BA0"]
["3VA2163-6HL32-0JL0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU320, LI, In=63A overload protection Ir=25A...63A short-circuit protection Ii=1.5...12 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",485.53,"ΤΕΜ",1,"LP",1,"3VA21636HL320JL0"]
["3VA2163-6KQ32-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU860, LSIG, In=63A overload protection Ir=25A...63A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.25...1 x In, tg=0.05-0.8s nut keeper kit",808.21,"ΤΕΜ",1,"LP",1,"3VA21636KQ320AA0"]
["3VA2163-7HN36-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU350, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In clamp connection",436.34999999999997,"ΤΕΜ",1,"LP",1,"3VA21637HN360AA0"]
["3VA2163-7MN36-0DC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 3-pole, motor protection ETU350M, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=3...15 x Ir, Ii=15 x In clamp connection undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",531.18999999999994,"ΤΕΜ",1,"LP",1,"3VA21637MN360DC0"]
["3VA2163-8HK46-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class L Icu=150kA @ 415V 4-pole, line protection ETU340, ELISA LI, In=63A overload protection Ir=25A...63A short-circuit protection Ii=15 x In N conductor protection adjustable (OFF, 100%) clamp connection",573.03,"ΤΕΜ",1,"LP",1,"3VA21638HK460AA0"]
["3VA2216-5MQ32-0AA0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU860M, LSIG, In=160A overload protection Ir=63A...160A short-circuit protection Isd=1.2..15x In, Ii=3..15x In gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit",797.18999999999994,"ΤΕΜ",1,"LP",1,"3VA22165MQ320AA0"]
["3VA2216-6JQ32-0AA0","circuit breaker 3VA2 IEC frame 250 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU560, LSIG, In=160A overload protection Ir=63A...160A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit",1115.28,"ΤΕΜ",1,"LP",1,"3VA22166JQ320AA0"]
["3VA2220-7MN32-0JA0","circuit breaker 3VA2 IEC frame 250 breaking capacity class C Icu=110kA @ 415V 3-pole, motor protection ETU350M, LSI, In=200A overload protection Ir=80A...200A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz",890.7,"ΤΕΜ",1,"LP",1,"3VA22207MN320JA0"]
["3VA2220-7MS32-0AH0","circuit breaker 3VA2 IEC frame 250 breaking capacity class C Icu=110kA @ 415V 3-pole, starter protection ETU310M, I, In=200A overload protection Ir=80A...200A short-circuit protection Ii=3...15 x In nut keeper kit 2 auxiliary switches HQ 1 trip alarm switch HQ",744.04,"ΤΕΜ",1,"LP",1,"3VA22207MS320AH0"]
["3VA2225-5HN32-0AD0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In nut keeper kit 3 auxiliary switches HQ",766.72,"ΤΕΜ",1,"LP",1,"3VA22255HN320AD0"]
["3VA2225-5HN42-0HH0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU350, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In N conductor protection adjustable (OFF, 50%, 100%) nut keeper kit shunt trip (STL) 12-30V DC; 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",1038.3799999999999,"ΤΕΜ",1,"LP",1,"3VA22255HN420HH0"]
["3VA2225-5JQ32-0JL0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU560, LSIG, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection, opt. w. external current transformer gr.-fault prot., can be sw. off Ig=0.2...1 x In= tg=0.05-0.8s nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",1150.28,"ΤΕΜ",1,"LP",1,"3VA22255JQ320JL0"]
["3VA2225-6HM42-0AA0","circuit breaker 3VA2 IEC frame 250 breaking capacity class H Icu=85kA @ 415V 4-pole, line protection ETU330, LIG, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...10 x In N conductor protection adjustable (OFF, 50%, 100%) ground-fault protection Ig=0.2...1 x In= tg=0.1/0.3s nut keeper kit",1175.4000000000001,"ΤΕΜ",1,"LP",1,"3VA22256HM420AA0"]
["3VA2225-6JP32-0AJ0","circuit breaker 3VA2 IEC frame 250 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU550, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer nut keeper kit 2 auxiliary switches HP 1 trip alarm switch HP",1034.23,"ΤΕΜ",1,"LP",1,"3VA22256JP320AJ0"]
["3VA2225-7HL32-0HC0","circuit breaker 3VA2 IEC frame 250 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU320, LI, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...10 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ",907.7,"ΤΕΜ",1,"LP",1,"3VA22257HL320HC0"]
["3VA2225-8HL32-0AH0","circuit breaker 3VA2 IEC frame 250 breaking capacity class L Icu=150kA @ 415V 3-pole, line protection ETU320, LI, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...10 x In nut keeper kit 2 auxiliary switches HQ 1 trip alarm switch HQ",999.4,"ΤΕΜ",1,"LP",1,"3VA22258HL320AH0"]
["3VA2325-5HL32-0AA0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...12 x In nut keeper kit",890.7,"ΤΕΜ",1,"LP",1,"3VA23255HL320AA0"]
["3VA2325-5MN32-0JL0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",1112.3799999999999,"ΤΕΜ",1,"LP",1,"3VA23255MN320JL0"]
["3VA2325-6HL32-0BC0","circuit breaker 3VA2 IEC frame 400 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU320, LI, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...12 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ",1118.3900000000001,"ΤΕΜ",1,"LP",1,"3VA23256HL320BC0"]
["3VA2325-6KP32-0BA0","circuit breaker 3VA2 IEC frame 400 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU850, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit undervoltage release (UVR) 24V DC",1360.26,"ΤΕΜ",1,"LP",1,"3VA23256KP320BA0"]
["3VA2340-5HL32-0BB0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=400A overload protection Ir=160A...400A short-circuit protection Ii=1.5...10 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HP",997.56,"ΤΕΜ",1,"LP",1,"3VA23405HL320BB0"]
["3VA2340-5HN42-0CA0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU350, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In N conductor protection adjustable (OFF, 50%, 100%) nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz",1311.06,"ΤΕΜ",1,"LP",1,"3VA23405HN420CA0"]
["3VA2340-5JP32-0KL0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU550, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6...10 x In, Ii=1.5 x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit shunt trip (STL) 220-250V DC; 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",1216.29,"ΤΕΜ",1,"LP",1,"3VA23405JP320KL0"]
["3VA2340-5KP32-0CH0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU850, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6...10 x In, Ii=1.5 x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",1326.31,"ΤΕΜ",1,"LP",1,"3VA23405KP320CH0"]
["3VA2340-6HN32-0HH0","circuit breaker 3VA2 IEC frame 400 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",1192.06,"ΤΕΜ",1,"LP",1,"3VA23406HN320HH0"]
["3VA2340-6JP42-0AJ0","circuit breaker 3VA2 IEC frame 400 breaking capacity class H Icu=85kA @ 415V 4-pole, line protection ETU550, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection adjustable (OFF, up to 100%) nut keeper kit circuit breaker 3VA2 IEC frame 400 breaking capacity class H Icu=85kA @ 415V 4-pole, line protection ETU550, LSI, In=400A overload protection 2 AUXILIARY SWITCH CHANGEOVER H 1 TRIP ALARM SWITCH CHANGEOVER",1708.46,"ΤΕΜ",1,"LP",1,"3VA23406JP420AJ0"]
["3VA2340-7HL32-0AA0","circuit breaker 3VA2 IEC frame 400 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU320, LI, In=400A overload protection Ir=160A...400A short-circuit protection Ii=1.5...10 x In nut keeper kit",1095.3799999999999,"ΤΕΜ",1,"LP",1,"3VA23407HL320AA0"]
["3VA2440-5HN32-0BL0","circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",1429.72,"ΤΕΜ",1,"LP",1,"3VA24405HN320BL0"]
["3VA2440-5MN32-0JL0","circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",1491.71,"ΤΕΜ",1,"LP",1,"3VA24405MN320JL0"]
["3VA2440-6HN32-0BH0","circuit breaker 3VA2 IEC frame 630 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ",1571.72,"ΤΕΜ",1,"LP",1,"3VA24406HN320BH0"]
["3VA2440-7JQ32-0BL0","circuit breaker 3VA2 IEC frame 630 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU560, LSIG, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6..10x In, Ii=1.5..15x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",1916.44,"ΤΕΜ",1,"LP",1,"3VA24407JQ320BL0"]
["3VA2450-6HK42-0AA0","circuit breaker 3VA2 IEC frame 630 breaking capacity class H Icu=85kA @ 415V 4-pole, line protection ETU340, ELISA LI, In=500A overload protection Ir=200A...500A short-circuit protection Ii=14 x In N conductor protection adjustable (OFF, 50%, 100%) nut keeper kit",1827.41,"ΤΕΜ",1,"LP",1,"3VA24506HK420AA0"]
["3VA2450-7MN32-0DA0","circuit breaker 3VA2 IEC frame 630 breaking capacity class C Icu=110kA @ 415V 3-pole, motor protection ETU350M, LSI, In=500A overload protection Ir=200A...500A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz",1912.07,"ΤΕΜ",1,"LP",1,"3VA24507MN320DA0"]
["3VA2463-5JP32-0AB0","circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU550, LSI, In=630A overload protection Ir=250A...630A short-circuit protection Isd=0.6..9 x In, Ii=1.5..9 x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit 2 auxiliary switches HP",1427.31,"ΤΕΜ",1,"LP",1,"3VA24635JP320AB0"]
["3VA2463-5KP32-0KA0","circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU850, LSI, In=630A overload protection Ir=250A...630A short-circuit protection Isd=0.6..9 x In, Ii=1.5..9 x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit shunt trip (STL) 220-250V DC; 208-277V AC",1553.35,"ΤΕΜ",1,"LP",1,"3VA24635KP320KA0"]
["3VA2463-6HN32-0AC0","circuit breaker 3VA2 IEC frame 630 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=630A overload protection Ir=250A...630A short-circuit protection Isd=1.5...9 x Ir, Ii=9 x In nut keeper kit 2 auxiliary switches HQ",1474.71,"ΤΕΜ",1,"LP",1,"3VA24636HN320AC0"]
["3VA2463-6JP32-0AA0","circuit breaker 3VA2 IEC frame 630 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU550, LSI, In=630A overload protection Ir=250A...630A short-circuit protection Isd=0.6..9x In, Ii=1.5..9x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit",1533.36,"ΤΕΜ",1,"LP",1,"3VA24636JP320AA0"]
["3VA2463-6KP32-0KC0","circuit breaker 3VA2 IEC frame 630 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU850, LSI, In=630A overload protection Ir=250A...630A short-circuit protection Isd=0.6..9 x In, Ii=1.5..9 x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit shunt trip (STL) 220-250V DC; 208-277V AC 2 auxiliary switches HQ",1730.41,"ΤΕΜ",1,"LP",1,"3VA24636KP320KC0"]
["3VA2463-7HN32-0JA0","circuit breaker 3VA2 IEC frame 630 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU350, LSI, In=630A overload protection Ir=250A...630A short-circuit protection Isd=1.5...9 x Ir, Ii=9 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz",1611.73,"ΤΕΜ",1,"LP",1,"3VA24637HN320JA0"]
["3VA2510-5HN32-0DL0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=1000A overload protection Ir=400A...1000A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",2525.1000000000004,"ΤΕΜ",1,"LP",1,"3VA25105HN320DL0"]
["3VA2510-7HM42-0AA0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class C Icu=110kA @ 415V 4-pole, line protection ETU330, LIG, In=1000A overload protection Ir=400A...1000A short-circuit protection Ii=1.5...10 x In N conductor protection adjustable (OFF, 50%, 100%) ground-fault protection Ig=0.2...1 x In= tg=0.1/0.3s nut keeper kit",4037.75,"ΤΕΜ",1,"LP",1,"3VA25107HM420AA0"]
["3VA2580-5HL32-0AE0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=800A overload protection Ir=320A...800A short-circuit protection Ii=1.5...12 x In nut keeper kit 4 auxiliary switches HQ",1736.4,"ΤΕΜ",1,"LP",1,"3VA25805HL320AE0"]
["3VA2580-5JP32-0AA0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU550, LSI, In=800A overload protection Ir=320A...800A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit",1805.39,"ΤΕΜ",1,"LP",1,"3VA25805JP320AA0"]
["3VA2580-6HN32-0AH0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=800A overload protection Ir=320A...800A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit 2 auxiliary switches HQ 1 trip alarm switch HQ",1918.08,"ΤΕΜ",1,"LP",1,"3VA25806HN320AH0"]
["3VA2580-7JP42-0AA0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class C Icu=110kA @ 415V 4-pole, line protection ETU550, LSI, In=800A overload protection Ir=320A...800A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) nut keeper kit",2787.6200000000003,"ΤΕΜ",1,"LP",1,"3VA25807JP420AA0"]
["3VA4112-6ED14-3AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class H 65kA @ 277 V 1-pole, line protection TM210, FTFM, In=125A overload protection Ir=125A fixed short circuit protection Ii=10 x In",272.69,"ΤΕΜ",1,"LP",36,"3VA41126ED143AA0"]
["3VA4120-5ED24-0AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class M 35kA @ 480 V 2-pole, line protection TM210,  FTFM, In=20A overload protection Ir=20A fixed short-circuit protection Ii=15 x In clamp connection",211.68,"ΤΕΜ",1,"LP",1,"3VA41205ED240AA0"]
["3VA4145-4ED14-3AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class S 25kA @ 277 V 1-pole, line protection TM210, FTFM, In=45A overload protection Ir=45A fixed short circuit protection Ii=10 x In",105.84,"ΤΕΜ",1,"LP",36,"3VA41454ED143AA0"]
["3VA4150-4ED34-0AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class S 25kA @ 480 V 3-pole, line protection TM210,  FTFM, In=50A overload protection Ir=50A fixed short-circuit protection Ii=10 x In clamp connection",204.33,"ΤΕΜ",1,"LP",1,"3VA41504ED340AA0"]
["3VA4180-5ED54-0AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class M 35kA @ 277 V 1-pole, line protection TM210,  FTFM, In=80A overload protection Ir=80A fixed short-circuit protection Ii=10 x In clamp connection",205.8,"ΤΕΜ",1,"LP",1,"3VA41805ED540AA0"]
["3VA4195-6ED54-0AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class H 65kA @ 277 V 1-pole, line protection TM210,  FTFM, In=15A overload protection Ir=15A fixed short-circuit protection Ii=20 x In clamp connection",206.54,"ΤΕΜ",1,"LP",1,"3VA41956ED540AA0"]
["3VA5112-4EC31-0AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class S 25kA @ 480V 3-pole, line protection TM230, FTAM, In=125A overload protection Ir=125A fixed short-circuit protection Ii=5...10 x In without connection",452.76,"ΤΕΜ",1,"LP",1,"3VA51124EC310AA0"]
["3VA5112-6ED21-1AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class H 65kA @ 480V 2-pole, line protection TM210, FTFM, In=125A overload protection Ir=125A fixed short-circuit protection Ii=10 x In UL 489 SB (naval), 50Β° C without connection",504.95,"ΤΕΜ",1,"LP",1,"3VA51126ED211AA0"]
["3VA5135-6ED21-1AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class H 65kA @ 480V 2-pole, line protection TM210, FTFM, In=35A overload protection Ir=35A fixed short-circuit protection Ii=10 x In UL 489 SB (naval), 50Β° C without connection",245.49,"ΤΕΜ",1,"LP",1,"3VA51356ED211AA0"]
["3VA5150-4ED31-0AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class S 25kA @ 480V 3-pole, line protection TM210, FTFM, In=50A overload protection Ir=50A fixed short-circuit protection Ii=10 x In without connection",204.33,"ΤΕΜ",1,"LP",1,"3VA51504ED310AA0"]
["3VA5160-5EC41-0AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class M 35kA @ 480 V 4-pole, line protection TM230, FTAM, In=60A overload protection Ir=60A fixed short-circuit protection Ii=5...10 x In N conductor unprotected without connection",302.08999999999997,"ΤΕΜ",1,"LP",1,"3VA51605EC410AA0"]
["3VA5180-6ED21-0AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class H 65kA @ 480V 2-pole, line protection TM210, FTFM, In=80A overload protection Ir=80A fixed short-circuit protection Ii=10 x In without connection",256.52,"ΤΕΜ",1,"LP",1,"3VA51806ED210AA0"]
["3VA5195-6ED11-1AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class H 50kA @ 277V 1-pole, line protection TM210, FTFM, In=15A overload protection Ir=15A fixed short-circuit protection Ii=20 x In UL 489 SB (naval), 50Β° C without connection",141.12,"ΤΕΜ",1,"LP",1,"3VA51956ED111AA0"]
["3VA5211-6GC41-0AA0","circuit breaker 3VA5 UL frame 250 breaking capacity class H 65kA @ 480V 4-pole, line protection TM230, FTAM, In=110A overload protection Ir=110A fixed short-circuit protection Ii=5...10 x In N conductor protection 100% without connection",1080.45,"ΤΕΜ",1,"LP",1,"3VA52116GC410AA0"]
["3VA5217-7GF41-0AA0","circuit breaker 3VA5 UL frame 250 breaking capacity class C 100kA @ 480V 4-pole, line protection TM240, ATAM, In=175A overload protection Ir=140A...175A short-circuit protection Ii=5...10 x In N conductor protection 100% without connection",1286.25,"ΤΕΜ",1,"LP",1,"3VA52177GF410AA0"]
["3VA5222-6GD41-0AA0","circuit breaker 3VA5 UL frame 250 breaking capacity class H 65kA @ 480V 4-pole, line protection TM210, FTFM, In=225A overload protection Ir=225A fixed short-circuit protection Ii=10 x In N conductor protection 100% without connection",1212.75,"ΤΕΜ",1,"LP",1,"3VA52226GD410AA0"]
["3VA5240-6ED31-1AA0","Circuit breaker 3VA5 UL Frame 250 Breaking capacity class H 65kA @ 480 V 3-pole, line protection TM210, FTFM, In=40A Overload protection Ir=40A fixed Short-circuit protection Ii=10 x In UL489 SB (naval), 50 deg. Cel Without connection",556.4,"ΤΕΜ",1,"LP",1,"3VA52406ED311AA0"]
["3VA5280-7EF31-0AA0","circuit breaker 3VA5 UL frame 250 breaking capacity class C 100kA @ 480V 3-pole, line protection TM240, ATAM, In=80A overload protection Ir=64A...80A short-circuit protection Ii=5...10 x In without connection",710.01,"ΤΕΜ",1,"LP",1,"3VA52807EF310AA0"]
["3VA5290-6GD41-0AA0","circuit breaker 3VA5 UL frame 250 breaking capacity class H 65kA @ 480V 4-pole, line protection TM210, FTFM, In=90A overload protection Ir=90A fixed short-circuit protection Ii=10 x In N conductor protection 100% without connection",764.4,"ΤΕΜ",1,"LP",1,"3VA52906GD410AA0"]
["3VA5325-7GC41-0AA0","CIRCUIT BREAKER 3VA5 UL FRAME 400 BREAKING CAPACITY CLASS  C 100kA @ 480 V 4POLE, LINE PROTECTION TM230,  FTAM, In=250A OVERLOAD PROTECTION IR=250A FIXED SHORT CIRCUIT PROTECTION II=5...10 X IN NEUTRAL PROTECTION 100% W/O CONNECTION",1558.2,"ΤΕΜ",1,"LP",1,"3VA53257GC410AA0"]
["3VA5445-5EF31-0AA0","CIRCUIT BREAKER 3VA5 UL Frame 600 BREAKING CAPACITY CLASS  M 35kA @ 480 V 3POLE, LINE PROTECTION TM240,  ATAM, In=450A WITHOUT OVERLOAD PROTECTION IR=315A ...450A SHORT CIRCUIT PROTECTION Ii=5...10 x In W/O CONNECTION",1587.6,"ΤΕΜ",1,"LP",1,"3VA54455EF310AA0"]
["3VA5570-6EC36-1AA0","circuit breaker 3VA5 UL frame 800 breaking capacity class  H 65kA @ 480 V 3-pole, line protection TM230,  FTAM, In=700A overload protection Ir=700A fixed short circuit protection Ii=5...10 x In",5343.45,"ΤΕΜ",1,"LP",1,"3VA55706EC361AA0"]
["3VA5580-6EC36-1AA0","circuit breaker 3VA5 UL frame 800 breaking capacity class  H 65kA @ 480 V 3-pole, line protection TM230,  FTAM, In=800A overload protection Ir=800A fixed short circuit protection Ii=5...10 x In",3748.5,"ΤΕΜ",1,"LP",1,"3VA55806EC361AA0"]
["3VA6110-6KL41-0AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class H 65kA @ 480V 4-pole, line protection ETU820, LI, In=100A overload protection Ir=40A...100A short-circuit protection Ii=1.5...12 x In without connection",1381.8,"ΤΕΜ",1,"LP",1,"3VA61106KL410AA0"]
["3VA6110-8JP31-0AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class L 150kA @ 480V 3-pole, line protection ETU550, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% without connection",1176,"ΤΕΜ",1,"LP",1,"3VA61108JP310AA0"]
["3VA6115-6JP41-0AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class H 65kA @ 480V 4-pole, line protection ETU550, LSI, In=150A overload protection Ir=60A...150A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection adjustable (OFF, up to 100%) without connection",1646.4,"ΤΕΜ",1,"LP",1,"3VA61156JP410AA0"]
["3VA6115-6KT31-2AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class H 65kA @ 480V 3-pole, line protection ETU856, LSI, In=150A overload protection Ir=60A...150A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer, up to 160% ground-fault alarm message via EFB300 or COM without connection",1918.35,"ΤΕΜ",1,"LP",1,"3VA61156KT312AA0"]
["3VA6140-6HM41-2AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class H 65kA @ 480V 4-pole, line protection ETU330, LIG, In=40A overload protection Ir=16A...40A short-circuit protection Ii=1.5...12 x In N conductor protection adjustable (OFF, 100%) ground-fault protection Ig=0.375...1 x In= tg=0.1/0.3s without connection",1021.65,"ΤΕΜ",1,"LP",1,"3VA61406HM412AA0"]
["3VA6140-7KT31-0AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class C 100kA @ 480V 3-pole, line protection ETU856, LSI, In=40A overload protection Ir=16A...40A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% ground-fault alarm message via EFB300 or COM without connection",1286.25,"ΤΕΜ",1,"LP",1,"3VA61407KT310AA0"]
["3VA6140-8HN41-2AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class L 150kA @ 480V 4-pole, line protection ETU350, LSI, In=40A overload protection Ir=16A...40A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In N conductor protection adjustable (OFF, 100%) without connection",970.2,"ΤΕΜ",1,"LP",1,"3VA61408HN412AA0"]
["3VA6210-6KM31-2DG0","circuit breaker 3VA6 UL frame 250 breaking capacity class H 65kA @ 480V 3-pole, line protection ETU830, LIG, In=100A overload protection Ir=40A...100A short-circuit protection Ii=1.5...12 x In ground-fault protection Ig=0.2...1 x In, tg=0.05-0.8s without connection",2234.4,"ΤΕΜ",1,"LP",1,"3VA62106KM312DG0"]
["3VA6210-8KL31-0AA0","circuit breaker 3VA6 UL frame 250 breaking capacity class L 150kA @ 480V 3-pole, line protection ETU820, LI, In=100A overload protection Ir=40A...100A short-circuit protection Ii=1.5...12 x In without connection",2109.4499999999998,"ΤΕΜ",1,"LP",1,"3VA62108KL310AA0"]
["3VA6225-5KM41-2AA0","circuit breaker 3VA6 UL frame 250 breaking capacity class M 35kA @ 480V 4-pole, line protection ETU830, LIG, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...10 x In ground-fault protection Ig=0.2...1 x In, tg=0.05-0.8s without connection",2440.1999999999998,"ΤΕΜ",1,"LP",1,"3VA62255KM412AA0"]
["3VA6225-6KP41-0AA0","circuit breaker 3VA6 UL frame 250 breaking capacity class H 65kA @ 480V 4-pole, line protection ETU850, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection adjustable (OFF, up to 100%) without connection",2249.1,"ΤΕΜ",1,"LP",1,"3VA62256KP410AA0"]
["3VA6325-5HM41-0AA0","circuit breaker 3VA6 UL frame 400 breaking capacity class M 35kA @ 480V 4-pole, line protection ETU330, LIG, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...12 x In N conductor protection adjustable (OFF, 50%, 100%) ground-fault protection Ig=0.2...1 x In= tg=0.1/0.3s without connection",2013.9,"ΤΕΜ",1,"LP",1,"3VA63255HM410AA0"]
["3VA6325-7JQ41-0AA0","circuit breaker 3VA6 UL frame 400 breaking capacity class C 100kA @ 480V 4-pole, line protection ETU560, LSIG, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) ground-fault protection Ig=0.2...1 x In= tg=0.05-0.8s without connection",2969.4,"ΤΕΜ",1,"LP",1,"3VA63257JQ410AA0"]
["3VA6325-7KT41-0AA0","circuit breaker 3VA6 UL frame 400 breaking capacity class C 100kA @ 480V 4-pole, line protection ETU856, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) ground-fault alarm message via EFB300 or COM without connection",2917.95,"ΤΕΜ",1,"LP",1,"3VA63257KT410AA0"]
["3VA6340-8KQ41-0AA0","circuit breaker 3VA6 UL frame 400 breaking capacity class L 150kA @ 480V 4-pole, line protection ETU860, LSIG, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection adjustable (OFF, up to 100%) ground-fault protection Ig=0.2...1 x In= tg=0.05-0.8s without connection",3410.4,"ΤΕΜ",1,"LP",1,"3VA63408KQ410AA0"]
["3VA6440-5JT41-2AA0","circuit breaker 3VA6 UL frame 600 breaking capacity class M 35kA @ 480V 4-pole, line protection ETU556, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) ground-fault alarm message via EFB300 or COM without connection",3528,"ΤΕΜ",1,"LP",1,"3VA64405JT412AA0"]
["3VA6440-6KQ41-0AA0","circuit breaker 3VA6 UL frame 600 breaking capacity class H 65kA @ 480V 4-pole, line protection ETU860, LSIG, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) ground-fault protection Ig=0.2...1 x In= tg=0.05-0.8s without connection",3675,"ΤΕΜ",1,"LP",1,"3VA64406KQ410AA0"]
["3VA6460-7HM41-0AA0","circuit breaker 3VA6 UL frame 600 breaking capacity class C 100kA @ 480V 4-pole, line protection ETU330, LIG, In=600A overload protection Ir=240A...600A short-circuit protection Ii=1.5...9 x In N conductor protection adjustable (OFF, 50%, 100%) ground-fault protection Ig=0.2...1 x In= tg=0.1/0.3s without connection",3270.75,"ΤΕΜ",1,"LP",1,"3VA64607HM410AA0"]
["3VA6560-5HL36-2AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  M 35kA @ 480 V 3-pole, line protection ETU320, LI, In=600A overload protection Ir=240A ...600A short circuit protection Ii=1,5...12 x In",2807.7,"ΤΕΜ",1,"LP",1,"3VA65605HL362AA0"]
["3VA6560-6HN46-0AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  H 65kA @ 480 V 4-pole, line protection ETU350,  LSI, In=600A overload protection Ir=240A ...600A short circuit protection Isd=1,5... 12 x Ir, Ii=12 x In",3138.45,"ΤΕΜ",1,"LP",1,"3VA65606HN460AA0"]
["3VA6560-7JQ32-0AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  C 100kA @ 480 V 3-pole, line protection ETU560,  LSIG, In=600A overload protection Ir=240A ...600A short circuit protection",3829.35,"ΤΕΜ",1,"LP",1,"3VA65607JQ320AA0"]
["3VA6580-5KQ42-0AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  M 35kA @ 480 V 4-pole, line protection ETU860,  LSIG, In=800A overload protection Ir=320A ...800A short circuit protection Isd=0,6..10x In, Ii=1,5..10x In",4630.5,"ΤΕΜ",1,"LP",1,"3VA65805KQ420AA0"]
["3VA6580-6HM36-2AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  H 65kA @ 480 V 3-pole, line protection ETU330, LIG, In=800A overload protection Ir=320A ...800A short circuit protection Ii=1,5...10 x In",4630.5,"ΤΕΜ",1,"LP",1,"3VA65806HM362AA0"]
["3VA6580-7HM32-0AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  C 100kA @ 480 V 3-pole, line protection ETU330,  LIG, In=800A overload protection Ir=320A ...800A short circuit protection Ii=1,5...10 x In",3520.65,"ΤΕΜ",1,"LP",1,"3VA65807HM320AA0"]
["3VA6610-7JP42-0AA0","circuit breaker 3VA6 UL frame 1000 breaking capacity class  C 100kA @ 480 V 4-pole, line protection ETU550,  LSI, In=1000A overload protection Ir=400A ...1000A short circuit protection Isd=0,6..10x In, Ii=1,5..10x In",6548.85,"ΤΕΜ",1,"LP",1,"3VA66107JP420AA0"]
["3VA9033-0SB10","cover frame 76.2x 45.65mm (WxH) accessory for: circuit breaker 3-pole without TMTU access 3VA5 125 front mounted rotary operator 3VA9157-0EK.. for 3VA5 125",19.990000000000002,"ΤΕΜ",1,"LP",1,"3VA90330SB10"]
["3VA9124-0KP10","plug-in unit conversion kit for MCCB accessory for: circuit breaker, 4-pole 3VA2 100/160/250",91.35,"ΤΕΜ",1,"LP",1,"3VA91240KP10"]
["3VA9137-0GA80","retaining bracket accessory for: 3VA5 125",17.920000000000002,"ΤΕΜ",1,"LP",1,"3VA91370GA80"]
["3VA9157-0FK25","door mounted rotary operator emergency-off IEC IP65 with door interlock accessory for: 3VA1 100/160",68.67,"ΤΕΜ",1,"LP",1,"3VA91570FK25"]
["3VA9187-0TB60","SLC adapter COM060, 24 V module accessory for: 3VA2 100/160/250 3VA6 150/250",45.12,"ΤΕΜ",1,"LP",5,"3VA91870TB60"]
["3VA9234-0JH11","box terminal w. control wire voltage tap-off 4 units accessory for: 3VA5 250",59.4,"ΤΕΜ",1,"LP",1,"3VA92340JH11"]
["3VA9257-0GX10","Aux switch module rot op mech 2 x leading to \"ON\" Accessory for: 3VA1 100/160/250",33.630000000000003,"ΤΕΜ",1,"LP",1,"3VA92570GX10"]
["3VA9271-0WF30","terminal cover extended 3-pole 1 unit accessory for: 3VA6 150/250 3VA5 250 plug-in/draw-out socket 3VA6 150/250",22.720000000000002,"ΤΕΜ",1,"LP",1,"3VA92710WF30"]
["3VA9277-0EK35","front mounted rotary operator emergency-off IP30 NEMA type 1,.. with door interlock and door open position accessory for: 3VA6 150/250 3VA5 250",113.19,"ΤΕΜ",1,"LP",1,"3VA92770EK35"]
["3VA9377-0NA10","external current transformer for N conductor, In = 400...600 , accessory for: 3VA2/6",585.9,"ΤΕΜ",1,"LP",1,"3VA93770NA10"]
["3VA9447-0HA20","motor operator 110-230V AC/110-250V DC accessory for: 3VA5/6 400/600",716.63,"ΤΕΜ",1,"LP",1,"3VA94470HA20"]
["3VA9477-0CB10","Operating Unit w/ Bowdencable Max-Flex Operator Switching mechanism only accessory for: 3VA5 400, 3VA5 600 3VA6 400, 3VA6 600",173.46,"ΤΕΜ",1,"LP",1,"3VA94770CB10"]
["3VA9671-0WE30","Terminal cover intermediate 3 pole; 1 pcs. accessory for: 3VA55/3VA65/3VA66",71.75,"ΤΕΜ",1,"LP",1,"3VA96710WE30"]
["3VA9978-0AB22","electrical alarm switch changeover contacts type HQ (7mm) accessory for: 3VA6",33.950000000000003,"ΤΕΜ",1,"LP",1,"3VA99780AB22"]
["3VA9988-0BA22","SHUNT TRIP FLEXIBLE 110-127 V AC 50/60 HZ ACCESSORY FOR 3VA10 up to 3VA14 and 3VA20 up to 3VA24",57.96,"ΤΕΜ",1,"LP",1,"3VA99880BA22"]
["3VL1703-1DD33-0AB1","circuit breaker VL160X N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection Electronic Trip Unit TM, LI In=32A, rated current Ir=25...32A, overload prot. II=300A, short-circuit prot. without auxiliary release Auxiliary switch mounting kit 2 AUX (1 NO + 1 NC)",429,"ΤΕΜ",1,"LP",1,"3VL17031DD330AB1"]
["3VL1704-1EA43-8TB1","circuit breaker VL160X N standard breaking capacity Icu=55kA, 415V AC 4-pole, line protection Electronic Trip Unit TM, LI In=40A, rated current Ir=40A, overload protection II=600A, short-circuit prot. N protected Shunt release 208...277 V AC Auxiliary switch mounting kit 2 AUX (1 NO + 1 NC)",641,"ΤΕΜ",1,"LP",1,"3VL17041EA438TB1"]
["3VL1706-1DA36-8TA0","circuit breaker VL160X N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection Electronic Trip Unit TM, LI In=63A, rated current Ir=63A, overload protection II=600A, short-circuit prot. with screw terminals Shunt release 208...277 V AC without auxiliary/alarm switch",455,"ΤΕΜ",1,"LP",1,"3VL17061DA368TA0"]
["3VL1708-2DA36-0AA0","circuit breaker VL160X H high breaking capacity Icu=70kA, 415V AC 3-pole, line protection Electronic Trip Unit TM, LI In=80A, rated current Ir=80A, overload protection II=1000A, short-circuit prot. with screw terminals without auxiliary release without auxiliary/alarm switch",397,"ΤΕΜ",1,"LP",1,"3VL17082DA360AA0"]
["3VL1712-2DD33-0AD1","circuit breaker VL160X H high breaking capacity Icu=70kA, 415V AC 3-pole, line protection Electronic Trip Unit TM, LI In=125A, rated current Ir=125A, overload protection II=1000A, short-circuit prot. without auxiliary release Auxiliary/alarm switch mounting kit 2 AUX (1 NO+1 NC)+1 AS (1 NO)",917,"ΤΕΜ",1,"LP",1,"3VL17122DD330AD1"]
["3VL1725-1EA43-0AA0","circuit breaker VL160X N standard breaking capacity Icu=55kA, 415V AC 4-pole, line protection Electronic Trip Unit TM, LI In=25A, rated current Ir=25A, overload protection II=300A, short-circuit prot. N protected without auxiliary release without auxiliary/alarm switch",447,"ΤΕΜ",1,"LP",1,"3VL17251EA430AA0"]
["3VL2515-1VM30-0AA0","circuit breaker VL150 UL type DG (cat no. NDK3G150) non-interchangeable frame, with circuit breaker approval acc. to UL 489 standard breaking capacity 3-pole; NEMA rating 35KA@480V and 18KA@600/347V (molded case circuit breaker) Electronic Trip Unit LCD ETU, LSIG TA=40Β°C 3 phases/4 lines In=150A, rated current ISD=1.25-10xIR, II=11X in short-circuit protection Ir=60-150A Electronic Trip Unit for line protection without connection accessories without auxiliary/alarm switch",2006,"ΤΕΜ",1,"LP",1,"3VL25151VM300AA0"]
["3VL2706-1EM46-0AA0","circuit breaker VL160N standard breaking capacity Icu=55kA, 415V AC 4-pole, line protection Electronic Trip Unit TM, LI In=63A, rated current Ir=50...63A, overload protection, II=300...600A, short-circuit protection N protected with screw terminals without auxiliary release without auxiliary/alarm switch",475,"ΤΕΜ",1,"LP",1,"3VL27061EM460AA0"]
["3VL2706-1SB33-0AD1","circuit breaker VL160N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection Electronic Trip Unit ETU10, LI In=63A, rated current IR=25...63A, overload protection, II=1.25 to 11xIN, short-circuit protection without auxiliary release Auxiliary/alarm switch mounting kit 2 AUX (1 NO+1 NC)+1 AS (1 NO)",807,"ΤΕΜ",1,"LP",1,"3VL27061SB330AD1"]
["3VL2706-2UN43-0AA0","circuit breaker VL160H high breaking capacity Icu=70kA, 415V AC 4-pole, line protection Electronic Trip Unit LCD ETU42, LSIG In=63A, rated current IR=25...63A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection N protected with ground-fault protection without auxiliary release without auxiliary/alarm switch",2186,"ΤΕΜ",1,"LP",1,"3VL27062UN430AA0"]
["3VL2706-3UN46-0AA0","circuit breaker VL160L very high breaking capacity Icu=100kA, 415V AC 4-pole, line protection Electronic Trip Unit LCD ETU42, LSIG In=63A, rated current IR=25...63A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection N protected with screw terminals without auxiliary release without auxiliary/alarm switch",2414,"ΤΕΜ",1,"LP",1,"3VL27063UN460AA0"]
["3VL2710-1EJ43-0AA0","circuit breaker VL160N standard breaking capacity Icu=55kA, 415V AC 4-pole, line protection Electronic Trip Unit TM, LI In=100A, rated current IR=80...100A, overload protection, II=500...1000A, short-circuit protection N unprotected without auxiliary release without auxiliary/alarm switch",604,"ΤΕΜ",1,"LP",1,"3VL27101EJ430AA0"]
["3VL2710-1MB33-2KA0","circuit breaker VL160N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection Electronic Trip Unit ETU10, LI In=100A, rated current IR=40...100A, overload protection, II=1.25 to 11xIN, short-circuit protection ETU communication-capable Undervoltage release 440...480 V AC without auxiliary/alarm switch",977,"ΤΕΜ",1,"LP",1,"3VL27101MB332KA0"]
["3VL2710-2EJ43-8TD1","circuit breaker VL160H high breaking capacity Icu=70kA, 415V AC 4-pole, line protection Electronic Trip Unit TM, LI In=100A, rated current IR=80...100A, overload protection, II=500...1000A, short-circuit protection N unprotected Shunt release 208...277 V AC Auxiliary/alarm switch mounting kit 2 AUX (1 NO+1 NC)+1 AS (1 NO)",926,"ΤΕΜ",1,"LP",1,"3VL27102EJ438TD1"]
["3VL2710-2UH33-0AA0","circuit breaker VL160H high breaking capacity Icu=70kA, 415V AC 3-pole, line protection Electronic Trip Unit LCD ETU40, LI/LS/LSI In=100A, rated current IR=40...100A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection without auxiliary release without auxiliary/alarm switch",1844,"ΤΕΜ",1,"LP",1,"3VL27102UH330AA0"]
["3VL2710-3SE33-0AA0","circuit breaker VL160L very high breaking capacity Icu=100kA, 415V AC 3-pole, line protection Electronic Trip Unit ETU20, LSI In=100A, rated current IR=40...100A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection without auxiliary release without auxiliary/alarm switch",1063,"ΤΕΜ",1,"LP",1,"3VL27103SE330AA0"]
["3VL2716-1DC33-2HA0","circuit breaker VL160N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection Electronic Trip Unit TM, LI In=160A, rated current IR=125...160A, overload protection, II=800...1600A, short-circuit protection Undervoltage release 220...250 V AC without auxiliary/alarm switch",1041,"ΤΕΜ",1,"LP",1,"3VL27161DC332HA0"]
["3VL2716-1SH33-0AA0","circuit breaker VL160N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection Electronic Trip Unit ETU22, LSIG 3 phases/4 lines with connecting cable In=160A, rated current IR=64...160A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection without auxiliary release without auxiliary/alarm switch",1510,"ΤΕΜ",1,"LP",1,"3VL27161SH330AA0"]
["3VL2716-2EJ43-8TA0","circuit breaker VL160H high breaking capacity Icu=70kA, 415V AC 4-pole, line protection Electronic Trip Unit TM, LI In=160A, rated current IR=125...160A, overload protection, II=800...1600A, short-circuit protection N unprotected Shunt release 208...277 V AC without auxiliary/alarm switch",1374,"ΤΕΜ",1,"LP",1,"3VL27162EJ438TA0"]
["3VL2716-3DC33-0AD1","circuit breaker VL160L very high breaking capacity Icu=100kA, 415V AC 3-pole, line protection Electronic Trip Unit TM, LI In=160A, rated current IR=125...160A, overload protection, II=800...1600A, short-circuit protection without auxiliary release Auxiliary/alarm switch mounting kit 2 AUX (1 NO+1 NC)+1 AS (1 NO)",1235,"ΤΕΜ",1,"LP",1,"3VL27163DC330AD1"]
["3VL2716-3NF46-0AA0","circuit breaker VL160L very high breaking capacity Icu=100kA, 415V AC 4-pole, line protection Electronic Trip Unit ETU20, LSI In=160A, rated current IR=64...160A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection N protected with screw terminals without auxiliary release ETU communication-capable without auxiliary/alarm switch",2125,"ΤΕΜ",1,"LP",1,"3VL27163NF460AA0"]
["3VL3125-2PH30-0AA0","circuit breaker VL250 UL; type FG (cat no. HFX3V250) non-interchangeable frame, with circuit breaker approval acc. to UL 489 high breaking capacity 3-pole, NEMA rating 65kA/480V, (molded case circuit breaker) Electronic Trip Unit ETU, LSIG TA=40Β°C 3 phases/4 lines In=250A, rated current ISD=1.5 to 10xIR, II=11X in short-circuit protection IR=70-250A Electronic Trip Unit for line protection without connection accessories without auxiliary release without auxiliary/alarm switch",2237,"ΤΕΜ",1,"LP",1,"3VL31252PH300AA0"]
["3VL3125-3VJ30-0AA0","circuit breaker VL250 UL type FG (cat no. LFX3K250) non-interchangeable frame, with circuit breaker approval acc. to UL 489 very high breaking capacity 3-pole; NEMA rating 100kA/480V and 25kA/600V (molded case circuit breaker) Electronic Trip Unit LCD ETU, LSIG-G with alarm TA=40Β°C 3 phases/4 lines In=250A, rated current ISD=1.25-10xIR, II=11X in short-circuit protection IR=70-250A Electronic Trip Unit for line protection without auxiliary release without auxiliary/alarm switch",3582,"ΤΕΜ",1,"LP",1,"3VL31253VJ300AA0"]
["3VL3720-1EC43-0AA0","circuit breaker VL250N standard breaking capacity Icu=55kA, 415V AC 4-pole, line protection Electronic Trip Unit TM, LI In=200A, rated current IR=160...200A, overload protection, II=1000...2000A, short-circuit protection N protected with box terminal without auxiliary release without auxiliary/alarm switch",1449,"ΤΕΜ",1,"LP",1,"3VL37201EC430AA0"]
["3VL3720-1SP36-0AD1","circuit breaker VL250N standard breaking capacity Icu=55kA, 415V AC 3-pole, motor/generator prot. Electronic Trip Unit ETU10M, LI In=200A, rated current IR=80...200A, overload protection, II=1.25 to 11xIN, short-circuit protection without auxiliary release Auxiliary/alarm switch mounting kit 2 AUX (1 NO+1 NC)+1 AS (1 NO)",1454,"ΤΕΜ",1,"LP",1,"3VL37201SP360AD1"]
["3VL3720-2TE43-0AA0","circuit breaker VL250H high breaking capacity Icu=70kA, 415V AC 4-pole, line protection Electronic Trip Unit ETU20, LSI In=200A, rated current IR=80...200A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection N unprotected without auxiliary release with box terminal without auxiliary/alarm switch",2213,"ΤΕΜ",1,"LP",1,"3VL37202TE430AA0"]
["3VL3720-3NN46-0AA0","circuit breaker VL250L very high breaking capacity Icu=100kA, 415V AC 4-pole, line protection Electronic Trip Unit ETU12, LIG In=200A, rated current IR=80...200A, overload protection, II=1.25 to 11xIN, short-circuit protection N protected without auxiliary release ETU communication-capable without auxiliary/alarm switch",3196,"ΤΕΜ",1,"LP",1,"3VL37203NN460AA0"]
["3VL3725-1DE36-0AD1","circuit breaker VL250N standard breaking capacity Icu=55kA, 415V AC 3-pole, non-auto. air circ. br. Electronic Trip Unit magnetic In=250A, rated current II=3500A, short-circuit protection without auxiliary release Auxiliary/alarm switch mounting kit 2 AUX (1 NO+1 NC)+1 AS (1 NO)",864,"ΤΕΜ",1,"LP",1,"3VL37251DE360AD1"]
["3VL3725-1MF33-0AA0","circuit breaker VL250N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection Electronic Trip Unit ETU12, LIGN 3 phases/4 lines In=250A, rated current IR=100...250A, overload protection, II=1.25 to 11xIN, short-circuit protection without auxiliary release with box terminal ETU communication-capable without auxiliary/alarm switch",2116,"ΤΕΜ",1,"LP",1,"3VL37251MF330AA0"]
["3VL3725-2SH33-0AA0","circuit breaker VL250H high breaking capacity Icu=70kA, 415V AC 3-pole, line protection Electronic Trip Unit ETU22, LSIG 3 phases/4 lines with connecting cable In=250A, rated current IR=100...250A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection without auxiliary release with box terminal without auxiliary/alarm switch",2081,"ΤΕΜ",1,"LP",1,"3VL37252SH330AA0"]
["3VL3725-3NA46-0AA0","circuit breaker VL250L very high breaking capacity Icu=100kA, 415V AC 4-pole, line protection Electronic Trip Unit ETU10, LIN In=250A, rated current IR=100...250A, overload protection, II=1.25 to 11xIN, short-circuit protection N protected without auxiliary release ETU communication-capable without auxiliary/alarm switch",2678,"ΤΕΜ",1,"LP",1,"3VL37253NA460AA0"]
["3VL4140-1VM30-0AA0","circuit breaker VL400 UL type JG (cat no. NJX3G400) non-interchangeable frame, with circuit breaker approval acc. to UL 489 standard breaking capacity 3-pole; NEMA rating 35kA/480V and 25kA/600V (molded case circuit breaker) Electronic Trip Unit LCD ETU, LSIG TA=40Β°C 3 phases/4 lines In=400A, rated current ISD=1.25-10xIR, II=11X in short-circuit protection IR=150-400A ETU for line protection without auxiliary release without auxiliary/alarm switch",3771,"ΤΕΜ",1,"LP",1,"3VL41401VM300AA0"]
["3VL4725-1DC36-2PD1","circuit breaker VL400N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection Electronic Trip Unit TM, LI In=250A, rated current IR=200...250A, overload protection, II=1200...2500A, short-circuit protection Undervoltage release 24 V DC Auxiliary/alarm switch mounting kit 2 AUX (1 NO+1 NC)+1 AS (1 NO)",1695,"ΤΕΜ",1,"LP",1,"3VL47251DC362PD1"]
["3VL4731-1SE36-2GD1","circuit breaker VL400N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection Electronic Trip Unit ETU20, LSI In=315A, rated current IR=128...315A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection Undervoltage release 110...127 V AC Auxiliary/alarm switch mounting kit 2 AUX (1 NO+1 NC)+1 AS (1 NO)",2395,"ΤΕΜ",1,"LP",1,"3VL47311SE362GD1"]
["3VL4731-2NH46-0AA0","circuit breaker VL400H high breaking capacity Icu=70kA, 415V AC 4-pole, line protection Electronic Trip Unit ETU22, LSIG In=315A, rated current IR=128...315A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection N protected without auxiliary release ETU communication-capable without auxiliary/alarm switch",4056,"ΤΕΜ",1,"LP",1,"3VL47312NH460AA0"]
["3VL4740-1EJ46-8TB1","circuit breaker VL400N standard breaking capacity Icu=55kA, 415V AC 4-pole, line protection trip unit TM, LI In=400A, rated current IR=320...400A, overload protection, II=2000...4000A, short-circuit protection N unprotected Shunt release 208...277 V AC Auxiliary switch mounting kit 2 AUX (1 NO + 1 NC)",2255,"ΤΕΜ",1,"LP",1,"3VL47401EJ468TB1"]
["3VL4740-3EJ46-0AA0","circuit breaker VL400L very high breaking capacity Icu=100kA, 415V AC 4-pole, line protection trip unit TM, LI In=400A, rated current IR=320...400A, overload protection, II=2000...4000A, short-circuit protection N unprotected without auxiliary release without auxiliary/alarm switch",2931,"ΤΕΜ",1,"LP",1,"3VL47403EJ460AA0"]
["3VL4860-2PB30-0AA0","circuit breaker VL400X UL; type LG (cat no. HLK3R600) non-interchangeable frame, with circuit breaker approval acc. to UL 489 high breaking capacity 3-pole, NEMA rating 65kA/480V and 18kA/600V (molded case circuit breaker) trip unit ETU, LI TA=40Β°C In=600A, rated current II=1.25 to 10xIN, short-circuit protection IR=200-600A ETU for line protection without connection accessories without auxiliary release without auxiliary/alarm switch",3539,"ΤΕΜ",1,"LP",1,"3VL48602PB300AA0"]
["3VL5731-1DC36-0AC1","circuit breaker VL630N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection trip unit TM, LI In=315A, rated current IR=250...315A, overload protection, II=1575...3150A, short-circuit protection without auxiliary release Auxiliary switch mounting kit 4 AUX (2 NO + 2 NC)",2171,"ΤΕΜ",1,"LP",1,"3VL57311DC360AC1"]
["3VL5763-1EJ46-0AA0","circuit breaker VL630N standard breaking capacity Icu=55kA, 415V AC 4-pole, line protection trip unit TM, LI In=630A, rated current IR=500...630A, overload protection, II=3250...6500A, short-circuit protection N unprotected without auxiliary release without auxiliary/alarm switch",2803,"ΤΕΜ",1,"LP",1,"3VL57631EJ460AA0"]
["3VL5763-2DC36-8TE1","circuit breaker VL630H high breaking capacity Icu=70kA, 415V AC 3-pole, line protection trip unit TM, LI In=630A, rated current IR=500...630A, overload protection, II=3250...6500A, short-circuit protection Shunt release 208...277 V AC Auxiliary/alarm switch mounting kit 2 AUX (1 NO+1 NC)+1 AS (1 NO)",2726,"ΤΕΜ",1,"LP",1,"3VL57632DC368TE1"]
["3VL6160-2PB30-0AA0","circuit breaker VL800 UL; type MG (cat no. HMX3R600) non-interchangeable frame, with circuit breaker approval acc. to UL 489 high breaking capacity 3-pole, NEMA rating 65kA/480V, (molded case circuit breaker) trip unit ETU, LI TA=40Β°C In=600A, rated current II=1.25 to 10xIN, short-circuit protection IR=200-600A ETU for line protection without connection accessories without auxiliary release without auxiliary/alarm switch",3762,"ΤΕΜ",1,"LP",1,"3VL61602PB300AA0"]
["3VL6780-1LA46-0AA0","circuit breaker VL800N standard breaking capacity Icu=55kA, 415V AC 4-pole, line protection trip unit ETU10, LI In=800A, rated current IR=320...800A, overload protection, II=1.25 to 8 xIN, short-circuit protection N protected shipbuilding certificate for LRS, DNV and gL without auxiliary release without auxiliary/alarm switch",5365,"ΤΕΜ",1,"LP",1,"3VL67801LA460AA0"]
["3VL7110-1KN30-0AA0","circuit breaker VL1200 UL; type NG (cat no. NNX3B100) non-interchangeable frame, with circuit breaker approval acc. to UL 489 standard breaking capacity 3-pole, NEMA rating 35kA/480V, (molded case circuit breaker) trip unit TM, LI TA=40Β°C In=< 1000A, rated current II=6000...10000A short-circuit protection IR=1000A ETU for line protection without connection accessories without auxiliary release without auxiliary/alarm switch",4876,"ΤΕΜ",1,"LP",1,"3VL71101KN300AA0"]
["3VL7710-1SE36-0AE1","circuit breaker VL1250N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection trip unit ETU20, LSI In=1000A, rated current IR=400...1000A, overload protection, ISD=1.5 to 10xIR, II=11 xIN short-circuit protection without auxiliary release Auxiliary/alarm switch mounting kit 2 AUX (1 NO+1 NC)+1 AS (1 NO)",4923,"ΤΕΜ",1,"LP",1,"3VL77101SE360AE1"]
["3VL7710-3SL36-0AA0","circuit breaker VL1250L very high breaking capacity Icu=100kA, 415V AC 3-pole, line protection trip unit ETU12, LIG 3 phases/3 lines In=1000A, rated current IR=400...1000A, overload protection, II=1.25 to 11xIN, short-circuit protection without auxiliary release without auxiliary/alarm switch",6607,"ΤΕΜ",1,"LP",1,"3VL77103SL360AA0"]
["3VL7712-2MF36-0AA0","circuit breaker VL1250H high breaking capacity Icu=70kA, 415V AC 3-pole, line protection trip unit ETU12, LIGN 3 phases/4 lines In=1250A, rated current IR=500...1250A, overload protection, II=1.25 to 10xIN, short-circuit protection without auxiliary release ETU communication-capable without auxiliary/alarm switch",7336,"ΤΕΜ",1,"LP",1,"3VL77122MF360AA0"]
["3VL8116-2KE30-0AA0","circuit breaker VL1600 UL; type PG (cat no. HPS3S160) non-interchangeable frame, with circuit breaker approval acc. to UL 489 high breaking capacity 3-pole, NEMA rating 65kA/480V, (molded case switch) trip unit magnetic TA=40Β°C In=< 1600A, rated current II=14000A short-circuit protection non-auto. air circuit breaker without connection accessories without auxiliary release without auxiliary/alarm switch",7901,"ΤΕΜ",1,"LP",1,"3VL81162KE300AA0"]
["3VL8716-1DE30-0AA0","circuit breaker VL1600N standard breaking capacity Icu=55kA, 415V AC 3-pole, non-auto. air circ. br. trip unit magnetic In=1600A, rated current II=14400A, short-circuit protection without auxiliary release without auxiliary/alarm switch",6628,"ΤΕΜ",1,"LP",1,"3VL87161DE300AA0"]
["3VL8716-3AA40-0AA0","circuit breaker VL1600L w/o Electronic Trip Unit very high breaking capacity Icu=100kA/415V AC, 4-pole In=< 1600A, rated current without auxiliary release with screw terminal connections for switching unit and ETU",5689,"ΤΕΜ",1,"LP",1,"3VL87163AA400AA0"]
["3VL9100-4TC30","accessory for VL160X, box terminals comprises 3 box terminals 3-pole",26.5,"ΤΕΜ",1,"LP",1,"3VL91004TC30"]
["3VL9210-6MS30","ETU VL160 3-pole, motor protection ETU30M, LI IR=40...100A, overload protection, TC=10A...30, time lag class II=6/8/11 xIN, short-circuit protection box terminal/screw terminal connections in scope of supply of sw. unit",615,"ΤΕΜ",1,"LP",1,"3VL92106MS30"]
["3VL9216-6LA40","ETU VL160, 4-pole, line protection ETU10, LI IR=64...160A, overload protection, II=1.25 to 11xIN, short-circuit protection, N protected box terminal/screw terminal connections in scope of supply of sw. unit shipbuilding certificate for LRS, DNV and gL",1265,"ΤΕΜ",1,"LP",1,"3VL92166LA40"]
["3VL9300-3JD01","Breaker VLVAR DEPTH red 1 3R 12 D/F-FR",241,"ΤΕΜ",1,"LP",1,"3VL93003JD01"]
["3VL9300-8CA31","accessory for VL150XUL-VL250UL, (CG frame FG frame) terminal cover IP30, extended, comprises 2 covers 3-pole",48.4,"ΤΕΜ",1,"LP",1,"3VL93008CA31"]
["3VL9320-8TC00","accessory for VL250, current transformer for overload protection of N conductor and for ground-fault protection In=200A",291,"ΤΕΜ",1,"LP",1,"3VL93208TC00"]
["3VL9400-1UT00","accessory for VL160X, VL160, VL250, VL400, undervoltage release 600V AC for installation on right",163,"ΤΕΜ",1,"LP",1,"3VL94001UT00"]
["3VL9400-3AS10","accessory for VL400, assembly kit, leading auxiliary switch 1 CO, from off to on 1.5m connecting cable",28.8,"ΤΕΜ",1,"LP",1,"3VL94003AS10"]
["3VL9400-4WC30","accessory for VL400, withdr. vers., assembly kit front connection, 3-pole",1106,"ΤΕΜ",1,"LP",1,"3VL94004WC30"]
["3VL9431-6LF40","ETU VL400, 4-pole, line protection ETU20, LSI IR=126...315A, overload protection, ISD=1.5 to 10xIR, II=11 xIN short-circuit protection, N protected screw terminal connections in scope of delivery of switching unit shipbuilding certificate for LRS, DNV and gL",1967,"ΤΕΜ",1,"LP",1,"3VL94316LF40"]
["3VL9440-6TF40","ETU VL400, 4-pole, line protection ETU20, LSI IR=160...400A, overload protection, ISD=1.5 to 10xIR, II=11 xIN short-circuit protection, N protected screw terminal connections in scope of delivery of switching unit",1703,"ΤΕΜ",1,"LP",1,"3VL94406TF40"]
["3VL9500-4TT40","accessory for VL630, connecting terminal plates f. flexible, flat Cu busbar with aux. conductor connection comprises 4 units, 4-pole",185,"ΤΕΜ",1,"LP",1,"3VL95004TT40"]
["3VL9600-3MJ01","accessory for VL800UL, (MG frame) mot. op. mech. w/ strd en. mech 24 VDC",1714,"ΤΕΜ",1,"LP",1,"3VL96003MJ01"]
["3VL9680-6TB40","ETU VL800, 4-pole, line protection ETU10, LI IR=320...800A, overload protection, II=1.25 to 8 xIN, short-circuit protection, screw terminal connections in scope of delivery of switching unit",1870,"ΤΕΜ",1,"LP",1,"3VL96806TB40"]
["3VL9712-6TF40","ETU VL1250, 4-pole, line protection ETU20, LSI IR=500...1250A, overload protection, ISD=1.5 to 9xIR, II=10xIN short-circuit protection, N protected screw terminal connections in scope of delivery of switching unit",4741,"ΤΕΜ",1,"LP",1,"3VL97126TF40"]
["3VL9800-1UU00","accessory for VL630, VL800, VL1250, VL1600, undervoltage release 48V DC for installation on right",204,"ΤΕΜ",1,"LP",1,"3VL98001UU00"]
["3VL9800-8CB40","accessory for VL1250, VL1600, terminal cover IP30 standard comprises 2 covers 4-pole",170,"ΤΕΜ",1,"LP",1,"3VL98008CB40"]
["3VL9816-6LF40","ETU VL1600, 4-pole, line protection ETU20, LSI, IR=640...1600A, overload protection, ISD=1.5 to 8 xIR, II=9 xIN short-circuit protection, N protected screw terminal connections in scope of delivery of switching unit shipbuilding certificate for LRS, DNV and gL",7637,"ΤΕΜ",1,"LP",1,"3VL98166LF40"]
["3VT1704-2EC46-0AA0","circuit breaker 3VT1 standard breaking capacity Icu=25kA, 415V AC 4-pole, line protection trip unit TM, LI In=40A rated current IR=32...40A overload protection II=200...400A, short-circuit protection N conductor unprotected without auxiliary release without auxiliary/alarm switch",273,"ΤΕΜ",1,"LP",1,"3VT17042EC460AA0"]
["3VT1792-2EJ46-0AA0","circuit breaker 3VT1 standard breaking capacity Icu=25kA, 415V AC 4-pole, line protection trip unit TM, LIN In=25A rated current IR=20...25A overload protection II=250...375A, short-circuit protection N conductor protected without auxiliary release without auxiliary/alarm switch",304,"ΤΕΜ",1,"LP",1,"3VT17922EJ460AA0"]
["3VT9215-4TD00","accessory for VT250 circular conductor terminal 25-150mm2 1 set = 1 unit",7.1,"ΤΕΜ",1,"LP",1,"3VT92154TD00"]
["3VT9300-3HG20","accessory for VT250, VT630 front panel for handle black degree of protection IP66",23.400000000000002,"ΤΕΜ",1,"LP",1,"3VT93003HG20"]
["3VT9500-3HA10","accessory for VT1000, VT1600 front mounted rotary op. w/o lock with shaft stub without knob add. shaft, masking plate and knob required",156,"ΤΕΜ",1,"LP",1,"3VT95003HA10"]
["3VW8112-0AA01","guide frame for 3WL10 - 3p rear vertical main circ. conn. equiv. to withdr. circ. breaker without frame accessory for circuit breaker 3WL10",1096,"ΤΕΜ",1,"LP",1,"3VW81120AA01"]
["3VW9011-0AT44","Adapter 3WL (Release 1) for TD400",168.01,"ΤΕΜ",1,"LP",1,"3VW90110AT44"]
["3VW9011-0BB10","locking mech to prevent opening in the cabinet door in ON pos. direct; on modified side panel or support of f.m. circ. br. accessory for circuit breaker 3WL10 / 3VA27",300,"ΤΕΜ",1,"LP",1,"3VW90110BB10"]
["3ZS1320-6CC00-0YL5","SIRIUS Soft Starter ES V15.1 Premium Software Update Service for Soft Starter ES 2007 Floating license for one user Engineering software, software and documentation on DVD License key on USB flash drive, Cl. A, 6 languages (de,en,it, fr,sp,cn) Executable in: Win 7 SP1 Win 10 - 64 bit; Win Server 2012 R2 Std, Win Server 2016 - 64 bit Reference hardware: 3RW44 Online functions via system interface and opt. DP/PN interface Content: Set (1xDVD + 1x USB)",221,"ΤΕΜ",1,"CP",1,"3ZS13206CC000YL5"]
["3ZS2711-0CC30-0YE0","power management software SENTRON powermanager V3.X Upgrade V2.0 Lean to V3.X device pack (10) license on USB flash drive software on CD-ROM for server and 1 client for Windows operating systems 4 languages (de, en/po/es)",832.53,"ΤΕΜ",1,"LP",1,"3ZS27110CC300YE0"]
["4AM2342-4TN00-0EA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,025 /0; UPRI(V):230+/-5%; USEC(V):24; ISEC(A):1,04; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-6 >UL/CSA-RECOGNIZED< >SAFETY ISOLATING TRANSFORMER<",84.8,"ΤΕΜ",1,"CP",1,"4AM23424TN000EA0"]
["4AM3442-5AT10-0FA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,1 /0,31; UPRI(V):400+/-5%; USEC(V):230; ISEC(A):0,43; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREWS/MOUNTING RAILS; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",122,"ΤΕΜ",1,"CP",1,"4AM34425AT100FA0"]
["4AM4042-5AT10-0FD0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,2 /0,85; UPRI(V):400+/-5%; USEC(V):230; ISEC(A):0,87; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP54; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",443,"ΤΕΜ",1,"CP",1,"4AM40425AT100FD0"]
["4AM4842-4TN00-0EA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,5 /2; UPRI(V):230+/-5%; USEC(V):24; ISEC(A):20,8; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-2, -2-6 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >SAFETY ISOLATING TRANSFORMER<",322,"ΤΕΜ",1,"CP",1,"4AM48424TN000EA0"]
["4AM5742-5FT10-0FC0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,85 /5; UPRI(V):500+/-5%; USEC(V):230; ISEC(A):3,7; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP23; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",758,"ΤΕΜ",1,"CP",1,"4AM57425FT100FC0"]
["4AM6542-5FT10-0FA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):2,5 /13,3; UPRI(V):500+/-5%; USEC(V):230; ISEC(A):10,9; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",1228,"ΤΕΜ",1,"CP",1,"4AM65425FT100FA0"]
["4AT3632-5AT10-0FC0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):5,6 /22,5; UPRI(V):400+/-5%; USEC(V):230; ISEC(A):24,4; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:55 /H; IP23; TYPE OF TERMINALS:SCREW CONNECTION; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",2807,"ΤΕΜ",1,"CP",1,"4AT36325AT100FC0"]
["4AV2400-2EB00-0A","POWER SUPPLY; PHASES:1; PN(KW):0,24; UPRI(V):400-230+/-15; USEC(V DC):24; ISEC(A DC):10/12 (60/40 CEL); F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; PROTECTION CL.:I; TA/ISOKL:60 /B; W(%):5; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-6, EN61131-2 >SAFETY ISOLATING TRANSFORMER<",644,"ΤΕΜ",1,"CP",1,"4AV24002EB000A"]
["4EP4003-0DS00","COMMUTATING CHOKE FOR CONVERTER; PHASES:3; UN1(V):400; ITHMAX 1(A) / F1(HZ):100 /50; I LN (A):90; UK(%):4; LN(MH):0,224; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:FLAT-TYPE TERMINAL; EN 61558-2-20 >CHOKE<",2703,"ΤΕΜ",1,"CP",1,"4EP40030DS00"]
["4EU2552-4UA00-0AA0","MAINS CHOKE F.FU; PHASES:3; UN1(V):480; ITHMAX 1(A) / F1(HZ):200 /60; I LN (A):180; UK(%):2; LN(MH):0,07; TA/ISOKL:40 /H; IP00; TYPE OF TERMINALS:FLAT-TYPE TERMINAL; EN 61558-2-20 >UL/CSA-RECOGNIZED< >CHOKE<",2204,"ΤΕΜ",1,"CP",1,"4EU25524UA000AA0"]
["4NC5327-2CE21","current transformer 600/5 A, 5 VA CL 1.0",55.47,"ΤΕΜ",1,"LP",1,"4NC53272CE21"]
["5SD7481-1","Surge arrester, Type 2, pluggable protective modules, UC 800 V AC, 1-pole, Varistor connected in series and gas-filled spark gap with remote signaling",192.79999999999998,"ΤΕΜ",1,"LP",1,"5SD74811"]
["5SG1702-1","NEOZED, fuse base, D02, 1-pole, 63 A, Un AC: 400 V, Un DC: 250 V",11.08,"ΤΕΜ",1,"LP",15,"5SG17021"]
["5SH5525","Auxiliary current switch for 5SG7230 and 3NW7430",9.99,"ΤΕΜ",1,"LP",1,"5SH5525"]
["5SJ4108-8HG41","Miniature circuit breaker 240 V 14kA, 1-pole, D, 8A, D=70 mm according to UL 489",214.76,"ΤΕΜ",1,"LP",1,"5SJ41088HG41"]
["5SJ4206-7HG41","Miniature circuit breaker 240 V 14kA, 2-pole, C, 6 A, D=70 mm according to UL 489",523.96,"ΤΕΜ",1,"LP",1,"5SJ42067HG41"]
["5SJ4210-7HG42","Circuit breaker 10kA, 2-pole, C, 10 A according to UL 489-480Y/277V",431.96,"ΤΕΜ",1,"LP",1,"5SJ42107HG42"]
["5SJ4308-8HG41","Miniature circuit breaker 240 V 4 kA, 3-pole, D, 8A, D=70 mm according to UL 489",871.92,"ΤΕΜ",1,"LP",1,"5SJ43088HG41"]
["5SL3132-7","Miniature circuit breaker 230/400 V 4.5 kA, 1-pole, C, 32 A",11.12,"ΤΕΜ",1,"LP",1,"5SL31327"]
["5SL3263-7","Miniature circuit breaker 400 V 4.5 kA, 2-pole, C, 63 A",53.28,"ΤΕΜ",1,"LP",1,"5SL32637"]
["5SL4106-6","Miniature circuit breaker 230/400 V 10kA, 1-pole, B, 6A",11.09,"ΤΕΜ",1,"LP",1,"5SL41066"]
["5SL4220-8","Miniature circuit breaker 400 V 10kA, 2-pole, D, 20 A",30,"ΤΕΜ",1,"LP",1,"5SL42208"]
["5SL4420-7","Miniature circuit breaker 400 V 10kA, 4-pole, C, 20 A",51.379999999999995,"ΤΕΜ",1,"LP",1,"5SL44207"]
["5SL4508-8","Miniature circuit breaker 230 V 10kA, 1+N-pole, D, 8A",24.46,"ΤΕΜ",1,"LP",1,"5SL45088"]
["5SL6140-6","Miniature circuit breaker 230/400 V 6kA, 1-pole, B, 40 A",7.34,"ΤΕΜ",1,"LP",1,"5SL61406"]
["5SL6514-7","Miniature circuit breaker 230 V 6kA, 1+N-pole, C, 0.3A",20.680000000000003,"ΤΕΜ",1,"LP",1,"5SL65147"]
["5SM2323-0","RC unit for 5SL4, 2-pole, typeΒ AC, In: 40 A, 30 mA, Un AC: 230 V",41.32,"ΤΕΜ",1,"LP",1,"5SM23230"]
["5SM2623-8","RC unit for 5SL4, 2-pole, type A, selective, In: 40 A, 300 mA, Un AC: 230 V",143.06,"ΤΕΜ",1,"LP",1,"5SM26238"]
["5SM3645-6","Residual current operated circuit breaker, 4-pole, type A, In: 125 A, 300 mA, Un AC: 400 V",668.52,"ΤΕΜ",1,"LP",1,"5SM36456"]
["5SP3863-2","Main miniature circuit breaker (SHU), 3x 1-pole, E 63A, 230/400 V Mounting on 40 mm busbars",598.98,"ΤΕΜ",1,"LP",1,"5SP38632"]
["5ST3602","Pin busbar, 10 mm2 connection: 12x 1-phase touch-safe",1.6300000000000001,"ΤΕΜ",1,"LP",10,"5ST3602"]
["5ST3702","Pin busbar touch-safe, 16 mm2 1-phase+AUX 214 mm long can be cut, with end caps",5.74,"ΤΕΜ",1,"LP",1,"5ST3702"]
["5ST3768-3","Connection terminal Central cable entry 690 V AC, 1000 V DC, 80 A IP20",3.26,"ΤΕΜ",1,"LP",10,"5ST37683"]
["5SU1324-1KK82","RCBO, 10 kA, 2P, Type AC, 30 mA, C-Char, In: 125 A, Un AC: 400 V",755.41,"ΤΕΜ",1,"LP",1,"5SU13241KK82"]
["5SU1353-1KL13","RCBO, 4.5 kA, 1P+N, Type AC, 30 mA, C-Char, In: 13 A, Un AC: 230 V, N left",93.37,"ΤΕΜ",1,"LP",1,"5SU13531KL13"]
["5SU1356-1KK08","RCBO, 6 kA, 1P+N, Type AC, 30 mA, C-Char, In: 8 A, Un AC: 230 V",142.73999999999998,"ΤΕΜ",1,"LP",1,"5SU13561KK08"]
["5SU1654-7KK10","RCBO, 10 kA, 1P+N, type A, 300 mA, C-Char, In: 10 A, Un AC: 230 V",187.64999999999998,"ΤΕΜ",1,"LP",1,"5SU16547KK10"]
["5SV1316-3KK10","RCBO compact 1P+N 6 kA type F 30 mA B10",232.32,"ΤΕΜ",1,"LP",1,"5SV13163KK10"]
["5SV3346-6BA","Residual current operated circuit breaker, 4-pole, type A, In: 63 A, 30 mA, Un AC: 400 V",203.57999999999998,"ΤΕΜ",1,"LP",1,"5SV33466BA"]
["5SV3642-6","Residual current operated circuit breaker, 4-pole, type A, In: 25 A, 300 mA, Un AC: 400 V",98.660000000000011,"ΤΕΜ",1,"LP",1,"5SV36426"]
["5SV4312-0","Residual current operated circuit breaker, 2-pole, Type AC, In: 25 A, 30 mA, Un AC: 230 V",58.11,"ΤΕΜ",1,"LP",1,"5SV43120"]
["5SV6016-6KP10","AFDD-MCB-combination 230V, 6kA, 1+N, B, 10A compact (1MW) pigtail",214.88,"ΤΕΜ",1,"LP",1,"5SV60166KP10"]
["5SV6316-6KP13","AFDD-RCBO-combination 230V, 30mA, type A 6kA, 1+N, B, 13A compact (1MW) pigtail",244.79999999999998,"ΤΕΜ",1,"LP",1,"5SV63166KP13"]
["5SY4108-8","Miniature circuit breaker 230/400 V 10kA, 1-pole, D, 8A, D=70 mm",33.269999999999996,"ΤΕΜ",1,"LP",1,"5SY41088"]
["5SY4115-8","Miniature circuit breaker 230/400 V 10kA, 1-pole, D, 1.6A, D=70 mm",33.269999999999996,"ΤΕΜ",1,"LP",1,"5SY41158"]
["5SY4225-7","Miniature circuit breaker 400 V 10kA, 2-pole, C, 25A, D=70 mm",20.950000000000003,"ΤΕΜ",1,"LP",1,"5SY42257"]
["5SY4303-7","Miniature circuit breaker 400 V 10kA, 3-pole, C, 3 A, D=70 mm",34.18,"ΤΕΜ",1,"LP",1,"5SY43037"]
["5SY4363-6KK11","Miniature circuit breaker 400 V 10kA, 3-pole, B, 63A for railway applications",1001,"ΤΕΜ",1,"LP",1,"5SY43636KK11"]
["5SY4440-6","Miniature circuit breaker 400 V 10kA, 4-pole, B, 40A, D=70 mm",82.76,"ΤΕΜ",1,"LP",1,"5SY44406"]
["5SY4606-6","Miniature circuit breaker 400 V 10kA, 3+N-pole, B, 6 A, D=70 mm",57.26,"ΤΕΜ",1,"LP",1,"5SY46066"]
["5SY5150-7","Circuit breaker Universal current 220 V DC 230/400 V AC 10kA, 1-pole, C, 50 A",29.55,"ΤΕΜ",1,"LP",1,"5SY51507"]
["5SY5408-7","Circuit breaker Universal current 880 V DC 400 V AC 10kA, 4-pole, C, 8A max. 1000 V DC",110.98,"ΤΕΜ",1,"LP",1,"5SY54087"]
["5SY6216-6","Miniature circuit breaker 400 V 6kA, 2-pole, B, 16A, D=70 mm",27.32,"ΤΕΜ",1,"LP",1,"5SY62166"]
["5SY6602-7","Miniature circuit breaker 400 V 6kA, 3+N-pole C, 2A, D=70 mm",52.33,"ΤΕΜ",1,"LP",1,"5SY66027"]
["5SY7104-7","Miniature circuit breaker 230/400 V 15kA, 1-pole, C, 4A, D=70 mm",15.19,"ΤΕΜ",1,"LP",1,"5SY71047"]
["5SY7303-8","Miniature circuit breaker 400 V 15kA, 3-pole, D, 3 A, D=70 mm",137.57,"ΤΕΜ",1,"LP",1,"5SY73038"]
["5SY7420-7","Miniature circuit breaker 400 V 15kA, 4-pole, C, 20 A, D=70 mm",71.350000000000009,"ΤΕΜ",1,"LP",1,"5SY74207"]
["5SY8114-8","Circuit breaker 230/400 V D=70 mm 25 kA according to EN 60947-2, 1P, D0.3",37.369999999999997,"ΤΕΜ",1,"LP",1,"5SY81148"]
["5SY8220-8BB08","Miniature circuit breaker 400 V 25kA, 2-pole, 20 A, D=70 mm only magnetic tripping",95.47,"ΤΕΜ",1,"LP",1,"5SY82208BB08"]
["5SY8425-7","Miniature circuit breaker 400 V D=70 mm 25 kA according to EN 60947-2, 4P, C25",92.09,"ΤΕΜ",1,"LP",1,"5SY84257"]
["5TA2155-0KK","DELTA switch device insert FM, two-circuit switch without claws 10A 250V",11.27,"ΤΕΜ",1,"LP",10,"5TA21550KK"]
["5TC1060","DELTA miro flush-mounted radio titanium white 230 V/50 Hz",290.25,"ΤΕΜ",1,"LP",1,"5TC1060"]
["5TC1555","DELTA style, titanium white Sun-blind control Complete unit 68x 68 mm",222.91,"ΤΕΜ",1,"LP",1,"5TC1555"]
["5TE4840","button, 1 NO+1 NO 20 A 2 keys red green, lamps 230 V",24.26,"ΤΕΜ",1,"LP",1,"5TE4840"]
["5TG1103-1","MIRO frame 3-fold wood cherry tree Color shade due to treatment",105.75,"ΤΕΜ",1,"LP",1,"5TG11031"]
["5TG1202-0","DELTA miro Frame 2-fold Authentic material glass crystal green without Siemens logo Dimensions 161x 90 mm",85.5,"ΤΕΜ",1,"LP",1,"5TG12020"]
["5TG1360-1","DELTA style, platinum metallic Cover plate for shutter toggle switch with symbol Up/Down",28.430000000000003,"ΤΕΜ",1,"LP",1,"5TG13601"]
["5TG2125","DELTA i-system carbon metallic Cover plate with shutter for support plates Modular jack connector",20.64,"ΤΕΜ",1,"LP",1,"5TG2125"]
["5TG4206","DELTA flaeche IP44, AP) Replacement window for light signal red",2.92,"ΤΕΜ",1,"LP",1,"5TG4206"]
["5TG4820","DELTA i-system HotelCard switch illuminated titanium white, 55x 55 mm",84.29,"ΤΕΜ",1,"LP",1,"5TG4820"]
["5TG5534-6WH","IRIS Frame 3-fold, vertical polar white",14.7,"ΤΕΜ",1,"LP",1,"5TG55346WH"]
["5TG6205","DELTA i-system titanium-white rocker switch Rocker switch for Series/double two-way switch for double pushbutton, 55x 55 mm",6.2,"ΤΕΜ",1,"LP",1,"5TG6205"]
["5TG6233","DELTA i-system carbon metallic Rocker switch with window, with label for Series/double two-way switch for pushbutton 2-fold Mid-position for double pushbutton, 55x 55 mm",14.4,"ΤΕΜ",1,"LP",1,"5TG6233"]
["5TG7987","DELTA profil, silver Rocker switch with shutter symbols for pushbutton 2-fold Mid-position 65x 65 mm",18.420000000000002,"ΤΕΜ",1,"LP",1,"5TG7987"]
["5TL1280-0","off switch 80A 2-pole",20.75,"ΤΕΜ",1,"LP",1,"5TL12800"]
["5TT4201-0","switching relay with 1 NO contact for 230V AC 16A control 230V AC",35.159999999999997,"ΤΕΜ",1,"LP",1,"5TT42010"]
["5TT5041-2","INSTA contactor with 3 NO contacts and 1 NC Contact for 230 V AC, 400V 40A Control AC/24 V DC",89.81,"ΤΕΜ",1,"LP",1,"5TT50412"]
["5TT5850-0","INSTA contactor with 4 NO contacts Contact for 230 V AC, 400V 63A Control 230 V AC",101.04,"ΤΕΜ",1,"LP",1,"5TT58500"]
["5UB1580","DELTA line SCHUKO socket outlet 250 V AC, 16A With screwless Connection terminals Solid plate 80 mm x 80 mm titanium white",8.2200000000000006,"ΤΕΜ",1,"LP",1,"5UB1580"]
["5UB1941","DELTA i-system SCHUKO socket outlet with increased touch protection with labeling field and operating display aluminum metallic, 55x 55 mm",32.559999999999995,"ΤΕΜ",1,"LP",1,"5UB1941"]
["5UH1213","DELTA i-system electrical white Cover plate with spring flap 55x 55 mm, with label for SCHUKO socket outlet",20.430000000000003,"ΤΕΜ",1,"LP",1,"5UH1213"]
["7KM1020-0BA01-1DA0","SENTRON PAC1020 96X96 mm Power Monitoring Device Panel mount type for measurement of electr. values Protocol: Modbus RTU With graphical display Un max: 400/230V 45-65Hz Input current 5A AC Power Supply 85V - 276V AC Terminal blocks",229,"ΤΕΜ",1,"LP",1,"7KM10200BA011DA0"]
["7KT1280-5MA07","SEM3 Split Core CT 1600:01 - 100 mA Secondary Output Current",394,"ΤΕΜ",1,"LP",1,"7KT12805MA07"]
["8GB5024-0KM","SIMBOX XL surface-mounting, without door 2-tier 2x 12 MW (14 MW) Safety class 2",62.16,"ΤΕΜ",1,"LP",1,"8GB50240KM"]
["8GF5688","Stab/SIKUS Universal Copper bar, flexible, L=2000 mm 24x 4x 1 mm 400 A, temp. 40 Β°C",332.86,"ΤΕΜ",1,"LP",1,"8GF5688"]
["8GK1052-2KK21","ALPHA 160, wall-mounted cabinet, Surface mounting, with distribution board panel, IP43, Protection class 2, H: 650 mm, W: 550 mm, T: 140 mm, RAL 9016",465.26,"ΤΕΜ",1,"LP",1,"8GK10522KK21"]
["8GK1122-5KA12","ALPHA 400, wall-mounted cabinet, IP43, Protection class 1, H: 1100 mm, W: 300 mm, T: 210 mm, RAL 9016",287.75,"ΤΕΜ",1,"LP",1,"8GK11225KA12"]
["8GK1133-5KA32","ALPHA 400, wall-mounted cabinet, IP55, Protection class 2, H: 1100 mm, W: 800 mm, T: 210 mm, RAL 9016",958.2,"ΤΕΜ",1,"LP",1,"8GK11335KA32"]
["8GK1323-8KP34","ALPHA 630, Floor-mounted cabinet, with open side wall, IP55, Protection class 1, H: 1950 mm, W: 800 mm, T: 320 mm, RAL 7035",1452.43,"ΤΕΜ",1,"LP",1,"8GK13238KP34"]
["8GK2325-6KK23","ALPHA 630 UNIVERSAL, Floor-mounted cabinet, IP55, Protection class 1, H: 1800 mm, W: 600 mm, T: 250 mm, RAL 7035, without door",615.33000000000004,"ΤΕΜ",1,"LP",1,"8GK23256KK23"]
["8GK4501-2KK22","ALPHA 400/630 DIN, Reserve section cover assembly kit with supports, H=300 W=500",45.51,"ΤΕΜ",1,"LP",1,"8GK45012KK22"]
["8GK4555-2KK12","ALPHA 400/630 DIN, Assembly kit for fuse switch disconnector 3NP4070, 2x NH00 to 160 A Support plate w. molded-plastic cover, H=300 W=250 DE, H=300 W=250",66.900000000000006,"ΤΕΜ",1,"LP",1,"8GK45552KK12"]
["8GK4731-4KK12","ALPHA 400/630 DIN Circuit breaker kit 1x 3VA23-24/400A/630A 3+4-pole H=600 mm W=250 mm, horizontal Installation for RCD module infeed side",186.75,"ΤΕΜ",1,"LP",1,"8GK47314KK12"]
["8GK6701-2KK33","ALPHA 630 Universal, Circuit breaker kit 1x 3VL160X/3VL160/3VL250 3+4-pole H=200 mm W=900 mm, Horizontal Installation, w. rotary operating mechanism",175.63,"ΤΕΜ",1,"LP",1,"8GK67012KK33"]
["8GK6736-6KK33","ALPHA 630 Universal Circuit breaker kit 5x 3VA10-11/100A/160A 3+4-pole H=600 mm W=900 mm, horizontal Installation for motorized operating mechanism for RCD module infeed side",298.26,"ΤΕΜ",1,"LP",1,"8GK67366KK33"]
["8GK6850-0KK04","ALPHA, mounting parts/set, stays, H: 2000 mm",115.76,"ΣΕΤ",1,"LP",1,"8GK68500KK04"]
["8GK9510-7KK31","ALPHA, door half, Left, IP55, H: 1100 mm, W: 525 mm, RAL 9016, type of protection 1 and 2",126.59,"ΤΕΜ",1,"LP",1,"8GK95107KK31"]
["8GK9521-8KK00","ALPHA partition horiz. Sheet steel",97.300000000000011,"ΤΕΜ",1,"LP",1,"8GK95218KK00"]
["8GK9601-4KK30","ALPHA 630 DIN, cover Height=600 mm, Width=750 mm, Closed Minimum order quantity 10 units",142.57,"ΤΕΜ",1,"LP",10,"8GK96014KK30"]
["8GK9607-2KK10","ALPHA 630 Universal, Section cover without cutouts H=400 mm, W=300 mm",54.879999999999995,"ΤΕΜ",1,"LP",1,"8GK96072KK10"]
["8GK9900-0KK34","ALPHA, Base, H: 100 mm, W: 800 mm, T: 320 mm, RAL 7035",219.95,"ΤΕΜ",1,"LP",1,"8GK99000KK34"]
["8GK9911-1KK02","ALPHA, cross arm, for busbar system, W: 750 mm, zinc-plated",95.940000000000012,"ΤΕΜ",1,"LP",1,"8GK99111KK02"]
["8MF1000-2HL","SIVACON, adapter, for the LΓΌtze wiring system, zinc-plated",120.19000000000001,"ΤΕΜ",1,"LP",1,"8MF10002HL"]
["8MF1000-2VC","SIVACON, Rotary handle insert, Square head",25.040000000000003,"ΤΕΜ",1,"LP",1,"8MF10002VC"]
["8MF1006-2UD20-0A","SIVACON, Roof, with Ventilation openings with Ventilation openings IP20, W: 1000 mm, T: 600 mm, zinc-plated",91.77000000000001,"ΤΕΜ",1,"LP",1,"8MF10062UD200A"]
["8MF1020-2HC03-0","SIVACON, mounting rail, serrated, U- shape L: 1200 mm, zinc-plated",42.61,"ΤΕΜ",1,"LP",1,"8MF10202HC030"]
["8MF1028-2UD30-0A","SIVACON, Roof, with Ventilation openings with Ventilation openings IP40, W: 1200 mm, T: 800 mm, zinc-plated",173.73999999999998,"ΤΕΜ",1,"LP",1,"8MF10282UD300A"]
["8MF1040-2UB12-0","SIVACON, base, Closed, IP55, T: 1000 mm, W: 400 mm, zinc-plated",96.45,"ΤΕΜ",1,"LP",1,"8MF10402UB120"]
["8MF1050-2UT15-1BA2","SIVACON, door, left, ventilated, IP20, H: 2000 mm, W: 500 mm, RAL 7035, Protection class 1",444.07,"ΤΕΜ",1,"LP",1,"8MF10502UT151BA2"]
["8MF1064-2GS40","SIVACON, Supporting structure, for standard Empty enclosure, H: 2000 mm, W: 600 mm, T: 400 mm, RAL 7035",707.62,"ΤΕΜ",1,"LP",1,"8MF10642GS40"]
["8MF1066-2AF30","SIVACON, compartment bottom, withdrawable, T: 600 mm, W: 600 mm, zinc-plated",304.89999999999998,"ΤΕΜ",1,"LP",1,"8MF10662AF30"]
["8MF1080-2AA12-0","SIVACON, mounting plate, Quick assembly with screws, perforated, H: 1000 mm, W: 800 mm, zinc-plated",175.75,"ΤΕΜ",1,"LP",1,"8MF10802AA120"]
["8MF1085-2UB52-0","SIVACON, base, with cutouts for flanges, IPXX, T: 500 mm, W: 800 mm, zinc-plated",60.96,"ΤΕΜ",1,"LP",1,"8MF10852UB520"]
["8MF1090-2CW","SIVACON, Transport bracket, heavy duty, W: 900 mm, RAL 7035",99.490000000000009,"ΣΕΤ",1,"LP",1,"8MF10902CW"]
["8MF1094-2VH","SIVACON, roof trough, for Increased degree of protection, IPX1, W: 900 mm, T: 400 mm, RAL 7035",150.97,"ΤΕΜ",1,"LP",1,"8MF10942VH"]
["8MF1111-0AA00-0AH7","SIVACON 2000mm x 600mm x 800mm",1680,"ΤΕΜ",1,"LP",1,"8MF11110AA000AH7"]
["8MF1111-0AA00-0AS2","SIVACON 2200mm x 800mm x 600mm",2355,"ΤΕΜ",1,"LP",1,"8MF11110AA000AS2"]
["8MF1111-0AA00-0AU0","SIVACON 2000mm x 600mm x 500mm",1935,"ΤΕΜ",1,"LP",1,"8MF11110AA000AU0"]
["8MF1111-0AA00-0BM7","SIVACON 2000mm x 800mm x 600mm",2475,"ΤΕΜ",1,"LP",1,"8MF11110AA000BM7"]
["8MF1111-0AA00-0BT4","SIVACON 1800mm x 600mm x 500mm",684.31,"ΤΕΜ",1,"LP",1,"8MF11110AA000BT4"]
["8MF1111-0AA00-0CF0","SIVACON 2000mm x 600mm x 500mm",2025,"ΤΕΜ",1,"LP",1,"8MF11110AA000CF0"]
["8MF1111-0AA00-0CM1","SIVACON 2000mm x 400mm x 800mm",1846.96,"ΤΕΜ",1,"LP",1,"8MF11110AA000CM1"]
["8MF1111-0AA00-0DC1","SIVACON 2000mm x 600mm x 500mm",2010,"ΤΕΜ",1,"LP",1,"8MF11110AA000DC1"]
["8MF1111-0AA00-0DQ1","SIVACON 2000mm x 800mm x 600mm",2355,"ΤΕΜ",1,"LP",1,"8MF11110AA000DQ1"]
["8MF1111-0AA00-0EA4","SIVACON 2000mm x 600mm x 500mm",2010,"ΤΕΜ",1,"LP",1,"8MF11110AA000EA4"]
["8MF1205-2AT30","SIVACON, partition, for vertical distribution of door, H: 2200 mm, RAL 7035, Protection class 1",71.960000000000008,"ΤΕΜ",1,"LP",1,"8MF12052AT30"]
["8MF1208-3VS4","SIVACON, Control panel Empty enclosure, according to IEC 62208, with ventilation openings, IP20, H: 2200 mm, W: 1000 mm, T: 800 mm",3214.02,"ΤΕΜ",1,"LP",1,"8MF12083VS4"]
["8MF1230-2UT15-0CA1","SIVACON, door, left, EMC, IP40, H: 2200 mm, W: 300 mm, RAL 7035, Protection class 1",802.5,"ΤΕΜ",1,"LP",1,"8MF12302UT150CA1"]
["8MF1250-2UT14-0BE2","SIVACON, door, right, inspection window, IP55, H: 2200 mm, W: 500 mm, RAL 7035, Protection class 1",568.21,"ΤΕΜ",1,"LP",1,"8MF12502UT140BE2"]
["8MF1270-2UT14-0BA2","SIVACON, door, right, IP55, H: 2200 mm, W: 450 mm, RAL 7035, Protection class 1",451.64,"ΤΕΜ",1,"LP",1,"8MF12702UT140BA2"]
["8MF1290-2UT14-2BA2","SIVACON, door, on the right, ventilated, IP40, H: 2200 mm, W: 900 mm, RAL 7035, Protection class 1",546.21,"ΤΕΜ",1,"LP",1,"8MF12902UT142BA2"]
["8MF1401-2HH","SIVACON, cable propping bar, D: 1000 mm, H: 40 mm, zinc-plated",52.22,"ΤΕΜ",1,"LP",1,"8MF14012HH"]
["8MF1804-2AK13-0","SIVACON, mounting plate, for cabinet side, perforated, D: 400 mm, H: 1800 mm, zinc-plated",137.66999999999999,"ΤΕΜ",1,"LP",1,"8MF18042AK130"]
["8MF1824-2GS30","SIVACON, Supporting structure, for standard Empty enclosure, H: 1800 mm, W: 1200 mm, T: 400 mm, zinc-plated",541.9,"ΤΕΜ",1,"LP",1,"8MF18242GS30"]
["8MF1850-2UT14-1BA2","SIVACON, door, on the right, ventilated, IP20, H: 1800 mm, W: 500 mm, RAL 7035, Protection class 1",428.06,"ΤΕΜ",1,"LP",1,"8MF18502UT141BA2"]
["8MF1870-2UT25-0CA1","SIVACON, door half, left, EMC, IP40, H: 1800 mm, W: 450 mm, RAL 7035, Protection class 1",732.92,"ΤΕΜ",1,"LP",1,"8MF18702UT250CA1"]
["8MF1888-3BS5","SIVACON, Control panel Empty enclosure, according to IEC 62208, IP55, H: 1800 mm, W: 800 mm, T: 800 mm",2441.7700000000004,"ΤΕΜ",1,"LP",1,"8MF18883BS5"]
["8MF1890-2UT15-1BA2","SIVACON, door, left, ventilated, IP20, H: 1800 mm, W: 900 mm, RAL 7035, Protection class 1",520.18999999999994,"ΤΕΜ",1,"LP",1,"8MF18902UT151BA2"]
["8MF2084-4R","standard cabinet 8MF2 HxWxD=2000x 800x 400 Installation: Side-by-side non-ventilated, assembled, welded IP40",2337.6600000000003,"ΤΕΜ",1,"LP",1,"8MF20844R"]
["8MF2208-3RB","standard cabinet 8MF2 HxWxD=2200x 1000x 800 Installation: Side-by-side ventilated, mounted, welded IP30",3399.7400000000002,"ΤΕΜ",1,"LP",1,"8MF22083RB"]
["8MF2294-4RB","standard cabinet 8MF2 HxWxD=2200x 900x 400 Installation: Side-by-side ventilated, mounted, welded IP40",2726.75,"ΤΕΜ",1,"LP",1,"8MF22944RB"]
["8MF2898-4RB","standard cabinet 8MF2 HxWxD=1800x 900x 800 Installation: Side-by-side ventilated, mounted, welded IP40",2752.7700000000004,"ΤΕΜ",1,"LP",1,"8MF28984RB"]
["8MF3111","Locking handle small with Lock (handle olive) Price is an additional price for Standard version",117.07000000000001,"ΤΕΜ",1,"LP",1,"8MF3111"]
["8MF3321","Double-wing door, asymmetrically separate, instead of rear panel HxW=2000x 1000 IP40 Price is an additional price for Standard version",812.25,"ΤΕΜ",1,"LP",1,"8MF3321"]
["8MF3365","Trim strip without Siemens logo, ochre, without indicator light cutout Price is an additional price for Standard version",52.669999999999995,"ΤΕΜ",1,"LP",1,"8MF3365"]
["8MF3866","compartment door instead of a standard door HxW=2000x 800 Price is an additional price for Standard version",866.75,"ΤΕΜ",1,"LP",1,"8MF3866"]
["8MF4078","Base plate without subdivision WxD=1200x 800",366.09999999999997,"ΤΕΜ",1,"LP",1,"8MF4078"]
["8MF4240","Trim strip without Siemens Logo anodized",85.38000000000001,"ΤΕΜ",1,"LP",1,"8MF4240"]
["8MF4825","19-inch compartment bottom D=400",227.09,"ΤΕΜ",1,"LP",1,"8MF4825"]
["8MF4901","Compact lamp 120V, 60Hz, 9 W KL025 02500.0-03",309,"ΤΕΜ",1,"LP",1,"8MF4901"]
["8MF5224-5E","Standard cabinet 8MF5 HxWxD=2200x 1200x 400 Installation: single non-ventilated, not mounted, screwed IP54,",4738.0200000000004,"ΤΕΜ",1,"LP",1,"8MF52245E"]
["8MF5886-4E","Standard cabinet 8MF5 HxWxD=1800x 800x 600 Installation: single non-ventilated, not mounted, screwed IP40",3218.44,"ΤΕΜ",1,"LP",1,"8MF58864E"]
["8MF6068-5E","Standard cabinet 8MF6 HxWxD=2000x 600x 800 Installation: single non-ventilated, assembled, welded IP54,",3631.8900000000003,"ΤΕΜ",1,"LP",1,"8MF60685E"]
["8MF6884-5E","Standard cabinet 8MF6 HxWxD=1800x 800x 400 Installation: single non-ventilated, assembled, welded IP54,",3296.5,"ΤΕΜ",1,"LP",1,"8MF68845E"]
["8MF6896-5R","Standard cabinet 8MF6 HxWxD=1800x 900x 600 Installation: Side-by-side non-ventilated, assembled, welded IP54,",3104.73,"ΤΕΜ",1,"LP",1,"8MF68965R"]
["8MR2150-5B","Semiconductor heater unit CSL 028 250 W, 230 V AC Screw mounting",246.5,"ΤΕΜ",1,"LP",1,"8MR21505B"]
["8MR2170-4F","120 V AC, 32-140 Β°F, 50-90%RF ETF012, 01230.9-00",341.05,"ΤΕΜ",1,"LP",1,"8MR21704F"]
["8MR6423-5LV30","Filter fan, Extract: W: 177 mm, H: 177 mm, RAL 7035, IP54, Airflow: 115 m3/h, Ue AC: 230 V",297.96999999999997,"ΤΕΜ",1,"LP",1,"8MR64235LV30"]
["8PQ1012-0BA01","SIVACON S4 Base corner pieces with front cover Height 100 mm Width 1200 mm",131,"ΤΕΜ",1,"LP",1,"8PQ10120BA01"]
["8PQ2010-6BA02","SIVACON S4 Cover ventilated Height 100 mm Width 600 mm",42.8,"ΤΕΜ",1,"LP",1,"8PQ20106BA02"]
["8PQ2022-6BA02","SIVACON S4 Upgrade IP55 Head compartment Height 225 mm Width 600 mm",66.5,"ΤΕΜ",1,"LP",1,"8PQ20226BA02"]
["8PQ2035-8BA16","SIVACON S4 Masking frame SENTRON 3VA 3VA10 (up to 100 A) 3-pole Upright mounting position Fixed mounting, Plug-in socket Number of switches 7 Height 350 mm Width 800 mm",94.8,"ΤΕΜ",1,"LP",1,"8PQ20358BA16"]
["8PQ2050-8BA15","SIVACON S4 Cover SENTRON 3VA 3VA13 (400A), 3VA14 (630A) 3VM13 (400A), 3VM14 (630A) 4-pole Fixed mounting Number of switches: 3 Mounting position: upright H: 500 mm W: 800 mm",135,"ΤΕΜ",1,"LP",1,"8PQ20508BA15"]
["8PQ2067-8BA01","SIVACON S4 Head compartment door Degree of protection IP40 Height 675 mm Width 800 mm",211,"ΤΕΜ",1,"LP",1,"8PQ20678BA01"]
["8PQ2197-0BA17","SIVACON S4, door, IP40, H: 1975 mm, W: 850 mm, Double-bit, right",386,"ΤΕΜ",1,"LP",1,"8PQ21970BA17"]
["8PQ2197-8BA12","SIVACON S4, door, IP55, H: 1975 mm, W: 800 mm, Double-bit, right",466,"ΤΕΜ",1,"LP",1,"8PQ21978BA12"]
["8PQ2302-8BA04","SIVACON S4 Base plate HSS bottom Degree of protection up to IP20 Closed Width 1200 mm Depth 800 mm",105,"ΤΕΜ",1,"LP",1,"8PQ23028BA04"]
["8PQ2420-0BA01","SIVACON S4 Rear wall Degree of protection IP4X Height 2000 mm Width 350 mm",132,"ΤΕΜ",1,"LP",1,"8PQ24200BA01"]
["8PQ3000-1BA55","SIVACON S4 Subdivision for the main busbar system Form 2B Main busbar front and rear Width 200 mm Depth 800 mm",67.2,"ΤΕΜ",1,"LP",1,"8PQ30001BA55"]
["8PQ4000-0BA76","SIVACON S4 Distribution busbar subdivision Form 2B without main busbar Depth 800 mm",364,"ΤΕΜ",1,"LP",1,"8PQ40000BA76"]
["8PQ5000-3BA61","SIVACON S4 EBS subdivision vertical for vertical distribution busbar Height 350 mm Width 800 mm",46.1,"ΤΕΜ",1,"LP",1,"8PQ50003BA61"]
["8PQ5000-4BA33","SIVACON S4 Subdivision 3WL Shape 4 Main busbar top Width 800 mm Depth 800 mm 0",408,"ΤΕΜ",1,"LP",1,"8PQ50004BA33"]
["8PQ6000-4BA44","SIVACON S4 EBS SENTRON 3VL Switch 3VL4 up to 400 A 3-pole, 3-pole+N, 4-pole Mounting position horizontal Fixed, Plug-in, Insert Number of switches 1 Height 250 mm Width 800 mm",85.8,"ΤΕΜ",1,"LP",1,"8PQ60004BA44"]
["8PQ6000-6BA38","SIVACON S4 EBS SENTRON 3VL Switches 3VL1 to 3VL3 3+N or 4-pole Mounting position horizontal connection system Direct operating mechanism through modular door Number of switches 1 Height 200 mm Width 600 mm",26.9,"ΤΕΜ",1,"LP",1,"8PQ60006BA38"]
["8PQ6000-8BA57","SIVACON S4 EBS SENTRON 3VA 3VA23 (400 A) 3-pole Upright mounting position Fixed mounting Number of switches 4 Height 350 mm Width 800 mm Branch height 450 mm",108,"ΤΕΜ",1,"LP",1,"8PQ60008BA57"]
["8PQ9400-0BA33","SIKUS/SIVACON Rubber cable entry Diameter 45 mm for cables 1x 14...38 mm",19.7,"ΤΕΜ",1,"LP",1,"8PQ94000BA33"]
["8UC7420-3BB","8UC7 handle with masking frame Spare part for 8UC6524-3BB44/8UC7424-3BB44 8UC6520-3BB Red handle masking frame yellow",111.82000000000001,"ΤΕΜ",1,"LP",1,"8UC74203BB"]
["8UD1741-0AC11","Handle with masking frame standard without tolerance compensation with door opening position Accessory for: 3VA1/2 1000 3VA5/6 800",84,"ΤΕΜ",1,"LP",1,"8UD17410AC11"]
["8US1061-5FP08","Busbar system Busbar center-to-center spacing 40 mm Device adapter, Width: 55 mm Bar thickness: 5+10 mm for circuit breaker with contactor 3R, S2 with 1 DIN rail 35 mm, up to 56 Length 242 mm",132,"ΤΕΜ",1,"LP",1,"8US10615FP08"]
["8US1251-5NS11","Device Adapter S0, 32A for 60mm Busbar system 45x200mm long special cables welded on AWG 10, 167 mm long with positioner",40.33,"ΤΕΜ",1,"LP",1,"8US12515NS11"]
["8WA1011-1BK11","Through-type terminal thermoplast Screw terminal on both sides Single terminal, blue, 10 mm Sz. 16",1.93,"ΤΕΜ",1,"LP",10,"8WA10111BK11"]
["8WA1822-7EF85","G fuse link DIN 41662 slow-response Low breaking capacity Rated continuous current 6.3 A",1.71,"ΤΕΜ",1,"LP",10,"8WA18227EF85"]
["8WA8348-0AA","inscription label, front, with 1, vertical, terminal width: 5 mm, H: 7 mm, white",8.3699999999999992,"ΤΕΜ",100,"LP",136,"8WA83480AA"]
["8WA8361-0AC","inscription label, front, with 1-40, vertical, terminal width: 5 mm, H: 7 mm, white",8.3699999999999992,"ΤΕΜ",100,"LP",204,"8WA83610AC"]
["8WB1002","inscription label, horizontal and vertical, W: 35 mm, white",964,"ΤΕΜ",1,"LP",1,"8WB1002"]
["8WD4420-0CF","Single-flash light element, w. built-in electronic flash, blue, 24 V DC, Diameter 70 mm",146,"ΤΕΜ",1,"CP",1,"8WD44200CF"]
["8WD4450-5AC","Continuous light element, with integrated LED, green, 230 V AC, Diameter 70 mm",73.699999999999989,"ΤΕΜ",1,"CP",1,"8WD44505AC"]
["8WH1000-0CG07","Through-type PE terminal with screw terminal Terminal width 6.2 mm Color green-yellow Cross-section: 4 mm2",3.1599999999999997,"ΤΕΜ",1,"LP",50,"8WH10000CG07"]
["8WH2000-0AF02","Through-type terminals with spring-loaded connection, Cross-section: 2.5 mm2, Width: 5.2mm, Color: red",0.82000000000000006,"ΤΕΜ",1,"LP",50,"8WH20000AF02"]
["8WH2000-1GG08","Fuse terminal for G fuse links 5x 20, 5x 25 and 5x 30 with 4 mm2 spring-loaded connection, Width: 6.2mm, Color: black",3.94,"ΤΕΜ",1,"LP",50,"8WH20001GG08"]
["8WH2020-5JF30","Two-tier terminals with illuminated indicator (15-30 V) with spring-loaded connection, Cross section: 0.08-2.5 mm2, Width: 5.2mm, Color: gray",6.63,"ΤΕΜ",1,"LP",50,"8WH20205JF30"]
["8WH2103-2BG00","Hybrid through-type terminal Screw and 2x spring-loaded connection Cross-section: 0.08-4 mm2, Width: 5.2mm, Color: gray",1.48,"ΤΕΜ",1,"LP",50,"8WH21032BG00"]
["8WH3000-6AE00","Isolating terminal with quick-connect technology Cross-section: 0.25-1.5 mm2, Width: 5.2mm, Color: gray",2.2999999999999998,"ΤΕΜ",1,"LP",50,"8WH30006AE00"]
["8WH8120-1AB45","Labeling plate, front, with 41-50 vertical, Terminal width: 4.2 mm, H: 10.5 mm, white",5.9799999999999995,"ΤΕΜ",100,"LP",100,"8WH81201AB45"]
["8WH8121-3AB55","Labeling plate, flat, with 51-60, vertical, Terminal width: 6.2 mm, H: 6.4 mm, white",5.6899999999999995,"ΤΕΜ",100,"LP",100,"8WH81213AB55"]
["8WH8202-5AA05","Labeling plate, front, horizontal und vertical, Terminal width: 10.2 mm, H: 10.5 mm, white",14.5,"ΤΕΜ",100,"LP",480,"8WH82025AA05"]
["8WH9000-4LA00","Cover for hybrid DG terminals 2.5 mm2, with 4 connection points, Plug-in connection on one side, Width: 2.2mm, Length 81 mm Color: gray",46.37,"ΤΕΜ",100,"LP",50,"8WH90004LA00"]
["8WH9010-0BC08","ALPHA, Shorting plug",6.29,"ΤΕΜ",1,"LP",10,"8WH90100BC08"]
["8WH9020-6AD10","Jumper plug 4 divisions, for cross links in the center of the terminal, 3-pole, Color: Siemens color",0.75,"ΤΕΜ",1,"LP",50,"8WH90206AD10"]
["8WH9020-6JC01","2 conn. combs 3.5Β mm blue",0.36,"ΤΕΜ",1,"LP",50,"8WH90206JC01"]
["8WH9120-0AA00","tap-off term., cross-sec. 10mm2 for high-current terminals, w/ 50mm2, fully insulated, enables one voltage tap up to a rated voltage of 1000 V, gray",5.04,"ΤΕΜ",1,"LP",10,"8WH91200AA00"]
["8WH9130-0AA00","shield terminal, for direct shield attachment on conductive mounting plates, diameter 3-8mm",5.35,"ΤΕΜ",1,"LP",10,"8WH91300AA00"]
["LZX:PT270615","Plug-in relay, 2 change-over contacts 115 V AC, also for LZS sockets",6.93,"ΤΕΜ",1,"CP",1,"LZX:PT270615"]
["US2:EP","Breaker Expansion Plug",916,"ΤΕΜ",1,"LP",1,"US2:EP"]
["US2:QJ23B125H00S01","Breaker QJ 3P 125A 240V 42kA ST",9758,"ΤΕΜ",1,"LP",1,"US2:QJ23B125H00S01"]
["US2:QJH23B080","Breaker QJ 3P 80A 240V 22kA",6601,"ΤΕΜ",1,"LP",1,"US2:QJH23B080"]
["US2:SEM3SCCT1200","SOLID CORE CT 1200:0.1",246,"ΤΕΜ",1,"LP",1,"US2:SEM3SCCT1200"]
["US2:SJD69200G","Breaker SJD 3P 200A 600V 25kA LIG TU",31875,"ΤΕΜ",1,"LP",1,"US2:SJD69200G"]
["US2:SND69120AGH","Breaker SND 3P 1200A 600V 25kA LIG 100",73913,"ΤΕΜ",1,"LP",1,"US2:SND69120AGH"]
["US2:SPD69160NT","Breaker SPD 3P 1600A 600V 25kA LSI TU",91551,"ΤΕΜ",1,"LP",1,"US2:SPD69160NT"]
["XPT:8PT10502","Compartment door W600 H2175 right IP42",886,"ΤΕΜ",1,"LP",1,"XPT:8PT10502"]
["XPT:8PT10722","Compartment door H1875 W8 right",654,"ΤΕΜ",1,"LP",1,"XPT:8PT10722"]
["XPT:8PT11320","Connecting bar reinforcement B",52.4,"ΤΕΜ",1,"LP",5,"XPT:8PT11320"]
["XPT:8PT12435","Top plate 1200/600 IPX1/2",151,"ΤΕΜ",1,"LP",5,"XPT:8PT12435"]
["XPT:8PT13005","Compartment door W800 H625 left",307,"ΤΕΜ",1,"LP",1,"XPT:8PT13005"]
["XPT:8PT1335","Door IP42 H750 W800 right",513,"ΤΕΜ",1,"LP",1,"XPT:8PT1335"]
["XPT:8PT1380","Door IP54 LT1 H22000 W800 on the right",809,"ΤΕΜ",1,"LP",1,"XPT:8PT1380"]
["XPT:8PT13967","Compartment door W1000 H2175 left IP42",1037,"ΤΕΜ",1,"LP",1,"XPT:8PT13967"]
["XPT:8PT14788","Partition 400",49.9,"ΤΕΜ",1,"LP",10,"XPT:8PT14788"]
["XPT:8PT14874","Compartment door IP54 H1300 B08",719,"ΤΕΜ",1,"LP",1,"XPT:8PT14874"]
["XPT:8PT15768","Compartment door H1300 B08 IP40 left",507,"ΤΕΜ",1,"LP",1,"XPT:8PT15768"]
["XPT:8PT16092","N-barrier",7.3,"ΤΕΜ",1,"LP",50,"XPT:8PT16092"]
["XPT:8PT17031","Partition 200x 600",27.700000000000003,"ΤΕΜ",1,"LP",10,"XPT:8PT17031"]
["XPT:8PT17143","End bus bar holder 3WL B600",96.1,"ΤΕΜ",1,"LP",5,"XPT:8PT17143"]
["XPT:8PT17585","Partition 800 horizontal left",30.400000000000002,"ΤΕΜ",1,"LP",20,"XPT:8PT17585"]
["XPT:8PT18386","Busbar holder WL1262 B600",77.5,"ΤΕΜ",1,"LP",5,"XPT:8PT18386"]
["XPT:8PT19305","Socket wrench SW17",230,"ΤΕΜ",1,"LP",1,"XPT:8PT19305"]
["XPT:8PT20998","Partition 1000 horiz. center",188,"ΤΕΜ",1,"LP",1,"XPT:8PT20998"]
["XPT:8PT21659","Device plate rear 400",47.300000000000004,"ΤΕΜ",1,"LP",10,"XPT:8PT21659"]
["XPT:8PT22061","Holder W800 coupling 3WL12",153,"ΤΕΜ",1,"LP",1,"XPT:8PT22061"]
["XPT:8PT22274","Empty mounting plate B800 H250",33.800000000000004,"ΤΕΜ",1,"LP",10,"XPT:8PT22274"]
["XPT:8PT227","Top plate B600/T600 O. cable entry",87.5,"ΤΕΜ",1,"LP",5,"XPT:8PT227"]
["XPT:8PT23226","Cover VL630 4P",69.399999999999991,"ΤΕΜ",1,"LP",5,"XPT:8PT23226"]
["XPT:8PT24136","Mounting plate VL800 B600",74.5,"ΤΕΜ",1,"LP",5,"XPT:8PT24136"]
["XPT:8PT24404","Section door W800 H2175 IP40",749,"ΤΕΜ",1,"LP",1,"XPT:8PT24404"]
["XPT:8PT24786","Cover IP30 CCS B850",86.6,"ΤΕΜ",1,"LP",5,"XPT:8PT24786"]
["XPT:8PT25015","Partition rear for B800",107,"ΤΕΜ",1,"LP",5,"XPT:8PT25015"]
["XPT:8PT2883","mounting bracket Busbar",757,"ΤΕΜ",100,"LP",100,"XPT:8PT2883"]
["XPT:8PT3011","Spacer 3VF6 4-pol. Plug-in socket",31.6,"ΤΕΜ",1,"LP",10,"XPT:8PT3011"]
["XPT:8PT3318","Busbar support 3NJ4",44,"ΤΕΜ",1,"LP",10,"XPT:8PT3318"]
["XPT:8PT360","Section door W800 H2175 ventilated R",565,"ΤΕΜ",1,"LP",1,"XPT:8PT360"]
["XPT:8PT4137","Cover 400",14.1,"ΤΕΜ",1,"LP",20,"XPT:8PT4137"]
["XPT:8PT4617","Vertical busbar holder top",97.5,"ΤΕΜ",1,"LP",5,"XPT:8PT4617"]
["XPT:8PT5079","Partition rear for B1200",65.099999999999994,"ΤΕΜ",1,"LP",5,"XPT:8PT5079"]
["XPT:8PT5398","Side wall left 300",24.200000000000003,"ΤΕΜ",1,"LP",10,"XPT:8PT5398"]
["XPT:8PT5537","Cover 150 mm 162.5/80 8UC61/62",43.6,"ΤΕΜ",1,"LP",10,"XPT:8PT5537"]
["XPT:8PT574","Device holder 575x 1000 MPC",96.699999999999989,"ΤΕΜ",1,"LP",5,"XPT:8PT574"]
["XPT:8PT5740","Side wall",21.900000000000002,"ΤΕΜ",1,"LP",20,"XPT:8PT5740"]
["XPT:8PT5741","Side wall",28.200000000000003,"ΤΕΜ",1,"LP",20,"XPT:8PT5741"]
["XPT:8PT5743","Duct cover",94.5,"ΤΕΜ",1,"LP",5,"XPT:8PT5743"]
["XPT:8PT5744","Holder bracket",11.299999999999999,"ΤΕΜ",1,"LP",30,"XPT:8PT5744"]
["XPT:8PT5745","Cover right",14.6,"ΤΕΜ",1,"LP",20,"XPT:8PT5745"]
["XPT:8PT5746","Cover left",13.5,"ΤΕΜ",1,"LP",30,"XPT:8PT5746"]
["XPT:8PT5747","Side bracket",42.1,"ΤΕΜ",1,"LP",10,"XPT:8PT5747"]
["XPT:8PT5757","Cover 300mm 202.5/80 8UC61/62",69.099999999999994,"ΤΕΜ",1,"LP",5,"XPT:8PT5757"]
["XPT:8PT5765","Busbar holder",36.300000000000004,"ΤΕΜ",1,"LP",10,"XPT:8PT5765"]
["XPT:8PT5768","Busbar holder",53,"ΤΕΜ",1,"LP",5,"XPT:8PT5768"]
["XPT:8PT5783","Mounting plate rear 100",14.1,"ΤΕΜ",1,"LP",30,"XPT:8PT5783"]
["XPT:8PT5785","Holder for cover 3NJ4",10.7,"ΤΕΜ",1,"LP",50,"XPT:8PT5785"]
["XPT:8PT5797","Side wall right 500",41.4,"ΤΕΜ",1,"LP",10,"XPT:8PT5797"]
["XPT:8PT5798","Side wall left 500",38.4,"ΤΕΜ",1,"LP",10,"XPT:8PT5798"]
["XPT:8PT5799","008/Mounting plate 500",50.6,"ΤΕΜ",1,"LP",10,"XPT:8PT5799"]
["XPT:8PT5807","Door 20X04 left, IP54,",628,"ΤΕΜ",1,"LP",1,"XPT:8PT5807"]
["XPT:8PT5808","Door 20X06 left IP54,",832,"ΤΕΜ",1,"LP",1,"XPT:8PT5808"]
["XPT:8PT5809","Door 20X08 left, IP54,",1025,"ΤΕΜ",1,"LP",1,"XPT:8PT5809"]
["XPT:8PT5815","Side wall right 600",54.300000000000004,"ΤΕΜ",1,"LP",10,"XPT:8PT5815"]
["XPT:8PT5816","Side wall left 600",51.7,"ΤΕΜ",1,"LP",10,"XPT:8PT5816"]
["XPT:8PT5817","Mounting plate 600",51.7,"ΤΕΜ",1,"LP",10,"XPT:8PT5817"]
["XPT:8PT5860","Mounting plate add-on 300",24.700000000000003,"ΤΕΜ",1,"LP",20,"XPT:8PT5860"]
["XPT:8PT5868","Mounting plate add-on 600",39.5,"ΤΕΜ",1,"LP",10,"XPT:8PT5868"]
["XPT:8PT5870","Mounting plate add-on 500",39.5,"ΤΕΜ",1,"LP",10,"XPT:8PT5870"]
["XPT:8PT5890","Vertical busbar holder",79.8,"ΤΕΜ",1,"LP",5,"XPT:8PT5890"]
["XPT:8PT5895","Holder",73.5,"ΤΕΜ",1,"LP",5,"XPT:8PT5895"]
["XPT:8PT5905","Insulating mat",77.899999999999991,"ΤΕΜ",1,"LP",5,"XPT:8PT5905"]
["XPT:8PT5909","Cover",142,"ΤΕΜ",1,"LP",5,"XPT:8PT5909"]
["XPT:8PT5920","Mounting plate 175x 600 3VF3 3P CC",43.6,"ΤΕΜ",1,"LP",10,"XPT:8PT5920"]
["XPT:8PT5925","Cover 1 3VF3 3P CCS3",38.4,"ΤΕΜ",1,"LP",10,"XPT:8PT5925"]
["XPT:8PT5926","Cover 2 3VF3 3P CCS3",24.200000000000003,"ΤΕΜ",1,"LP",20,"XPT:8PT5926"]
["XPT:8PT593","Busbar clipper",432,"ΤΕΜ",100,"LP",100,"XPT:8PT593"]
["XPT:8PT594","Clipper plate",57.6,"ΤΕΜ",1,"LP",5,"XPT:8PT594"]
["XPT:8PT5943","Lever",536,"ΤΕΜ",100,"LP",100,"XPT:8PT5943"]
["XPT:8PT5944","Bars",243,"ΤΕΜ",100,"LP",150,"XPT:8PT5944"]
["XPT:8PT595","Clipper plate U",50.6,"ΤΕΜ",1,"LP",10,"XPT:8PT595"]
["XPT:8PT5950","standard",6.81,"ΤΕΜ",1,"LP",50,"XPT:8PT5950"]
["XPT:8PT5951","standard",312,"ΤΕΜ",100,"LP",100,"XPT:8PT5951"]
["XPT:8PT5952","Standard 200 3KL53",360,"ΤΕΜ",100,"LP",100,"XPT:8PT5952"]
["XPT:8PT5953","Bars 4KT8",488,"ΤΕΜ",100,"LP",100,"XPT:8PT5953"]
["XPT:8PT5954","Standard 600 4KT12",6.15,"ΤΕΜ",1,"LP",100,"XPT:8PT5954"]
["XPT:8PT5955","Bars 4KT12 3VF6",9.56,"ΤΕΜ",1,"LP",50,"XPT:8PT5955"]
["XPT:8PT5957","Sheet bottom",8.07,"ΤΕΜ",1,"LP",50,"XPT:8PT5957"]
["XPT:8PT5958","Adapter 3RV",128,"ΤΕΜ",1,"LP",30,"XPT:8PT5958"]
["XPT:8PT5959","Mounting bracket SD",17.3,"ΤΕΜ",1,"LP",20,"XPT:8PT5959"]
["XPT:8PT5965","Busbar holder",34,"ΤΕΜ",1,"LP",10,"XPT:8PT5965"]
["XPT:8PT5966","mounting bracket",9.7899999999999991,"ΤΕΜ",1,"LP",50,"XPT:8PT5966"]
["XPT:8PT597","Transformer bar holder 800",113,"ΤΕΜ",1,"LP",5,"XPT:8PT597"]
["XPT:8PT5972","Cover rear 1 m",8.49,"ΤΕΜ",1,"LP",50,"XPT:8PT5972"]
["XPT:8PT5973","Cover rear 1.5 m",11.799999999999999,"ΤΕΜ",1,"LP",30,"XPT:8PT5973"]
["XPT:8PT5974","Cover rear 2 m",13,"ΤΕΜ",1,"LP",30,"XPT:8PT5974"]
["XPT:8PT5975","Additional cover form 4B",70.899999999999991,"ΤΕΜ",1,"LP",5,"XPT:8PT5975"]
["XPT:8PT5976","Additional cover form 4B",37.300000000000004,"ΤΕΜ",1,"LP",10,"XPT:8PT5976"]
["XPT:8PT598","Transformer bar holder 800",76.099999999999994,"ΤΕΜ",1,"LP",5,"XPT:8PT598"]
["XPT:8PT599","Transformer bar holder 800",113,"ΤΕΜ",1,"LP",5,"XPT:8PT599"]
["XPT:8PT5997","INSTR PANEL 100 without plug",524,"ΤΕΜ",100,"LP",100,"XPT:8PT5997"]
["XPT:8PT5998","INSTR PANEL 150 without plug",8.41,"ΤΕΜ",1,"LP",50,"XPT:8PT5998"]
["XPT:8PT600","Transformer bar holder 800",71.599999999999994,"ΤΕΜ",1,"LP",5,"XPT:8PT600"]
["XPT:8PT6005","Mounting plate add-on 200",17.900000000000002,"ΤΕΜ",1,"LP",20,"XPT:8PT6005"]
["XPT:8PT601","Transformer bar holder 800",103,"ΤΕΜ",1,"LP",5,"XPT:8PT601"]
["XPT:8PT6017","Adapter bracket",10.7,"ΤΕΜ",1,"LP",30,"XPT:8PT6017"]
["XPT:8PT602","Transformer bar holder 800",67.599999999999994,"ΤΕΜ",1,"LP",5,"XPT:8PT602"]
["XPT:8PT6032","Arc fault barrier 4000",127,"ΤΕΜ",1,"LP",5,"XPT:8PT6032"]
["XPT:8PT606","Transformer bar holder 600",90.1,"ΤΕΜ",1,"LP",5,"XPT:8PT606"]
["XPT:8PT6071","Cover 2 3VF6 3P 4P CCS3",25.8,"ΤΕΜ",1,"LP",10,"XPT:8PT6071"]
["XPT:8PT608","Transformer bar holder 600",90.1,"ΤΕΜ",1,"LP",5,"XPT:8PT608"]
["XPT:8PT6084","Reinforcement",118,"ΤΕΜ",1,"LP",5,"XPT:8PT6084"]
["XPT:8PT6086","Device holder H500 OFPD",102,"ΤΕΜ",1,"LP",5,"XPT:8PT6086"]
["XPT:8PT6087","Device holder 275 mm",39.5,"ΤΕΜ",1,"LP",10,"XPT:8PT6087"]
["XPT:8PT610","Transformer bar holder 600",84.6,"ΤΕΜ",1,"LP",5,"XPT:8PT610"]
["XPT:8PT6104","Mounting plate 400",33.800000000000004,"ΤΕΜ",1,"LP",10,"XPT:8PT6104"]
["XPT:8PT6117","Mounting plate add-on 400",55.4,"ΤΕΜ",1,"LP",5,"XPT:8PT6117"]
["XPT:8PT6121","Mounting plate 150",29.2,"ΤΕΜ",1,"LP",10,"XPT:8PT6121"]
["XPT:8PT6122","Mounting plate 100",23.700000000000003,"ΤΕΜ",1,"LP",20,"XPT:8PT6122"]
["XPT:8PT613","Connection bar holder 800",169,"ΤΕΜ",1,"LP",1,"XPT:8PT613"]
["XPT:8PT614","Connection bar holder 600",133,"ΤΕΜ",1,"LP",5,"XPT:8PT614"]
["XPT:8PT6147","Support 40x 10",30.400000000000002,"ΤΕΜ",1,"LP",10,"XPT:8PT6147"]
["XPT:8PT615","Connecting bar reinforcement",50.6,"ΤΕΜ",1,"LP",10,"XPT:8PT615"]
["XPT:8PT6150","Positioning aid crank",50.6,"ΤΕΜ",1,"LP",5,"XPT:8PT6150"]
["XPT:8PT616","Mounting bracket field bars",324,"ΤΕΜ",100,"LP",100,"XPT:8PT616"]
["XPT:8PT6161","Cover 1 3VF5 3P_4P CCS3",75.699999999999989,"ΤΕΜ",1,"LP",5,"XPT:8PT6161"]
["XPT:8PT6162","Cover 2 3VF5 3P_4P CCS3",24.700000000000003,"ΤΕΜ",1,"LP",10,"XPT:8PT6162"]
["XPT:8PT6163","Mounting plate 375x 600 3VF5 3P_4",78.3,"ΤΕΜ",1,"LP",5,"XPT:8PT6163"]
["XPT:8PT619","Support 1 field bar FE",54.300000000000004,"ΤΕΜ",1,"LP",5,"XPT:8PT619"]
["XPT:8PT620","Support 2 field bar FE",33.800000000000004,"ΤΕΜ",1,"LP",10,"XPT:8PT620"]
["XPT:8PT621","Support 3 field bar FE",13,"ΤΕΜ",1,"LP",20,"XPT:8PT621"]
["XPT:8PT6219","Mounting plate 275x 600 3VF4 3P 4P",55.800000000000004,"ΤΕΜ",1,"LP",10,"XPT:8PT6219"]
["XPT:8PT6220","Cover 1 3VF4 3P 4P CCS3",75.3,"ΤΕΜ",1,"LP",5,"XPT:8PT6220"]
["XPT:8PT6221","Cover 2 3VF4 3P 4P CCS3",24.700000000000003,"ΤΕΜ",1,"LP",20,"XPT:8PT6221"]
["XPT:8PT6225","Cover 1 3VF3 4P CCS3",38.800000000000004,"ΤΕΜ",1,"LP",10,"XPT:8PT6225"]
["XPT:8PT6226","Cover 2 3VF3 4P CCS3",24.700000000000003,"ΤΕΜ",1,"LP",20,"XPT:8PT6226"]
["XPT:8PT6244","Mounting plate 275x 600 3VF3 4P CC",55.800000000000004,"ΤΕΜ",1,"LP",10,"XPT:8PT6244"]
["XPT:8PT6284","Partition 4B 3WN1 800 top",165,"ΤΕΜ",1,"LP",5,"XPT:8PT6284"]
["XPT:8PT6285","Partition 4B 3WN1 800 top 2",38.6,"ΤΕΜ",1,"LP",10,"XPT:8PT6285"]
["XPT:8PT6288","Sealing angle B06",34,"ΤΕΜ",1,"LP",20,"XPT:8PT6288"]
["XPT:8PT6290","Sealing angle B04",32.299999999999997,"ΤΕΜ",1,"LP",20,"XPT:8PT6290"]
["XPT:8PT6292","Sealing angle B08",35.700000000000003,"ΤΕΜ",1,"LP",20,"XPT:8PT6292"]
["XPT:8PT6293","Sealing angle H20",45,"ΤΕΜ",1,"LP",20,"XPT:8PT6293"]
["XPT:8PT6299","Mounting plate 3VF6",62.4,"ΤΕΜ",1,"LP",5,"XPT:8PT6299"]
["XPT:8PT632","Base compartment door H175 left",83.8,"ΤΕΜ",1,"LP",1,"XPT:8PT632"]
["XPT:8PT634","Compartment door W600XH200 UF",85.699999999999989,"ΤΕΜ",1,"LP",1,"XPT:8PT634"]
["XPT:8PT635","Compartment door width 600 x height 400 UF",148,"ΤΕΜ",1,"LP",1,"XPT:8PT635"]
["XPT:8PT636","Compartment door W600XH500 MPC",192,"ΤΕΜ",1,"LP",1,"XPT:8PT636"]
["XPT:8PT6367","busbar reinforcement",23.1,"ΤΕΜ",1,"LP",20,"XPT:8PT6367"]
["XPT:8PT637","Compartment door W600XH600 MPC",223,"ΤΕΜ",1,"LP",1,"XPT:8PT637"]
["XPT:8PT6370","Connecting bar reinforcement",78.599999999999994,"ΤΕΜ",1,"LP",5,"XPT:8PT6370"]
["XPT:8PT6379","Support 4-pol. 40x 10",34.9,"ΤΕΜ",1,"LP",10,"XPT:8PT6379"]
["XPT:8PT6404","Mounting plate 375x 600 SENTRON J",73.399999999999991,"ΤΕΜ",1,"LP",5,"XPT:8PT6404"]
["XPT:8PT6405","Cover SENTRON JF CCS3",40.5,"ΤΕΜ",1,"LP",10,"XPT:8PT6405"]
["XPT:8PT6406","Cover plate JF CCS3",65.099999999999994,"ΤΕΜ",1,"LP",5,"XPT:8PT6406"]
["XPT:8PT641","Front plate 3VF6 4-pole",93.399999999999991,"ΤΕΜ",1,"LP",5,"XPT:8PT641"]
["XPT:8PT6418","Spindle nut M12",9.56,"ΤΕΜ",1,"LP",50,"XPT:8PT6418"]
["XPT:8PT642","Device holder 3VF6 4-pole",36,"ΤΕΜ",1,"LP",10,"XPT:8PT642"]
["XPT:8PT6432","Cover SENTLF CCS3",40.9,"ΤΕΜ",1,"LP",10,"XPT:8PT6432"]
["XPT:8PT6445","Mounting plate 275x 600 SENTRON",53,"ΤΕΜ",1,"LP",10,"XPT:8PT6445"]
["XPT:8PT6446","Insulating plate SENTRON FF CCS3",54.9,"ΤΕΜ",1,"LP",5,"XPT:8PT6446"]
["XPT:8PT6447","Cover SENTRON FF CCS3",39.4,"ΤΕΜ",1,"LP",10,"XPT:8PT6447"]
["XPT:8PT6452","Base panel 02X04",53,"ΤΕΜ",1,"LP",6,"XPT:8PT6452"]
["XPT:8PT6453","Base panel 02X08",89.6,"ΤΕΜ",1,"LP",6,"XPT:8PT6453"]
["XPT:8PT6455","Base panel 02x 10",108,"ΤΕΜ",1,"LP",6,"XPT:8PT6455"]
["XPT:8PT6456","Base panel 02x 12",127,"ΤΕΜ",1,"LP",6,"XPT:8PT6456"]
["XPT:8PT648","Brace L=420",24.700000000000003,"ΤΕΜ",1,"LP",20,"XPT:8PT648"]
["XPT:8PT649","Brace L=620",32.6,"ΤΕΜ",1,"LP",10,"XPT:8PT649"]
["XPT:8PT650","Brace L=820",46.2,"ΤΕΜ",1,"LP",10,"XPT:8PT650"]
["XPT:8PT6501","Cover 3VL160 3-pole",51,"ΤΕΜ",1,"LP",10,"XPT:8PT6501"]
["XPT:8PT6502","Cover 3VL160 4-pole",63.5,"ΤΕΜ",1,"LP",5,"XPT:8PT6502"]
["XPT:8PT6503","Cover 3VL630 3-pole",88.2,"ΤΕΜ",1,"LP",5,"XPT:8PT6503"]
["XPT:8PT6504","Cover 3VL630 4-pole",105,"ΤΕΜ",1,"LP",5,"XPT:8PT6504"]
["XPT:8PT6505","Mounting plate 3VL160 3-pole",18.600000000000001,"ΤΕΜ",1,"LP",20,"XPT:8PT6505"]
["XPT:8PT6506","Mounting plate 3VL160 4-pole",21.400000000000002,"ΤΕΜ",1,"LP",20,"XPT:8PT6506"]
["XPT:8PT6507","Mounting plate 3VL630 3-pole",28.200000000000003,"ΤΕΜ",1,"LP",10,"XPT:8PT6507"]
["XPT:8PT6508","Mounting plate 3VL630 4-pole",25.8,"ΤΕΜ",1,"LP",10,"XPT:8PT6508"]
["XPT:8PT651","Brace L=1720",66.8,"ΤΕΜ",1,"LP",6,"XPT:8PT651"]
["XPT:8PT6515","Mounting plate 275x 600 3NP52 CCS3",55.800000000000004,"ΤΕΜ",1,"LP",10,"XPT:8PT6515"]
["XPT:8PT6516","Cover 1 3NP52 CCS3",38.800000000000004,"ΤΕΜ",1,"LP",10,"XPT:8PT6516"]
["XPT:8PT6517","Cover 2 3NP52 CCS3",24.200000000000003,"ΤΕΜ",1,"LP",20,"XPT:8PT6517"]
["XPT:8PT652","Support for crossbar B600",42.5,"ΤΕΜ",1,"LP",10,"XPT:8PT652"]
["XPT:8PT653","Front cover for W600",78.3,"ΤΕΜ",1,"LP",5,"XPT:8PT653"]
["XPT:8PT6539","standard",6.81,"ΤΕΜ",1,"LP",50,"XPT:8PT6539"]
["XPT:8PT654","Front cover for W1200 LI",79.8,"ΤΕΜ",1,"LP",5,"XPT:8PT654"]
["XPT:8PT6540","Guide bracket",377,"ΤΕΜ",100,"LP",100,"XPT:8PT6540"]
["XPT:8PT6548","Mounting plate add-on 150",15.799999999999999,"ΤΕΜ",1,"LP",20,"XPT:8PT6548"]
["XPT:8PT655","Front cover for W1200",79.399999999999991,"ΤΕΜ",1,"LP",5,"XPT:8PT655"]
["XPT:8PT656","Connecting bar holder",49.9,"ΤΕΜ",1,"LP",10,"XPT:8PT656"]
["XPT:8PT659","Device holder 1675x 800 MPC",234,"ΤΕΜ",1,"LP",1,"XPT:8PT659"]
["XPT:8PT6597","Mounting plate 375x 600 3NP53 CCS",78.3,"ΤΕΜ",1,"LP",5,"XPT:8PT6597"]
["XPT:8PT6598","Cover 1 3NP53 CCS3",27.6,"ΤΕΜ",1,"LP",10,"XPT:8PT6598"]
["XPT:8PT6599","Cover 2 3NP53 CCS3",27.1,"ΤΕΜ",1,"LP",10,"XPT:8PT6599"]
["XPT:8PT6601","angle Mounting plate installation",10.7,"ΤΕΜ",1,"LP",30,"XPT:8PT6601"]
["XPT:8PT6611","Mounting plate 20x10",282,"ΤΕΜ",1,"LP",1,"XPT:8PT6611"]
["XPT:8PT6615","Slide rail T10 Mounting plate",25.8,"ΤΕΜ",1,"LP",20,"XPT:8PT6615"]
["XPT:8PT662","Support bottom T800",51,"ΤΕΜ",1,"LP",10,"XPT:8PT662"]
["XPT:8PT663","Support bottom T1000",65.699999999999989,"ΤΕΜ",1,"LP",5,"XPT:8PT663"]
["XPT:8PT664","Center support for B1200",135,"ΤΕΜ",1,"LP",5,"XPT:8PT664"]
["XPT:8PT665","Frame rail for B1200",67.3,"ΤΕΜ",1,"LP",5,"XPT:8PT665"]
["XPT:8PT666","Support bottom T600",39.4,"ΤΕΜ",1,"LP",10,"XPT:8PT666"]
["XPT:8PT6664","Cover 1 3NP54 CCS3",32.1,"ΤΕΜ",1,"LP",10,"XPT:8PT6664"]
["XPT:8PT6665","Cover 2 3NP54 CCS3",28.200000000000003,"ΤΕΜ",1,"LP",10,"XPT:8PT6665"]
["XPT:8PT667","Center crossbar front",55.4,"ΤΕΜ",1,"LP",10,"XPT:8PT667"]
["XPT:8PT6672","Partition horizontal left UV",234,"ΤΕΜ",1,"LP",1,"XPT:8PT6672"]
["XPT:8PT6673","Partition horizontal left HV",354,"ΤΕΜ",1,"LP",1,"XPT:8PT6673"]
["XPT:8PT668","Support cross beam movable, B80",41,"ΤΕΜ",1,"LP",10,"XPT:8PT668"]
["XPT:8PT6683","Mounting plate 500",65.699999999999989,"ΤΕΜ",1,"LP",5,"XPT:8PT6683"]
["XPT:8PT6684","Mounting plate 500",55.800000000000004,"ΤΕΜ",1,"LP",5,"XPT:8PT6684"]
["XPT:8PT669","Right center front holder",26.5,"ΤΕΜ",1,"LP",10,"XPT:8PT669"]
["XPT:8PT6698","Movable hinge",8.49,"ΤΕΜ",1,"LP",50,"XPT:8PT6698"]
["XPT:8PT6699","Hinge",6.81,"ΤΕΜ",1,"LP",50,"XPT:8PT6699"]
["XPT:8PT670","Left front cover for B600",152,"ΤΕΜ",1,"LP",1,"XPT:8PT670"]
["XPT:8PT6702","Cover 3NJ4 160A",88.2,"ΤΕΜ",1,"LP",5,"XPT:8PT6702"]
["XPT:8PT6703","Cover 300 mm 162_5/180 8UC63/66",69.099999999999994,"ΤΕΜ",1,"LP",5,"XPT:8PT6703"]
["XPT:8PT6709","Frame profile screwed 2",147,"ΤΕΜ",1,"LP",20,"XPT:8PT6709"]
["XPT:8PT671","Eight front cover for B600",147,"ΤΕΜ",1,"LP",5,"XPT:8PT671"]
["XPT:8PT6710","Frame profile screwed 2",146,"ΤΕΜ",1,"LP",20,"XPT:8PT6710"]
["XPT:8PT6712","Transverse spar screwed 04",53,"ΤΕΜ",1,"LP",12,"XPT:8PT6712"]
["XPT:8PT6713","Transverse spar screwed 06",49.2,"ΤΕΜ",1,"LP",12,"XPT:8PT6713"]
["XPT:8PT6714","Transverse spar screwed 08",59.4,"ΤΕΜ",1,"LP",12,"XPT:8PT6714"]
["XPT:8PT6716","Transverse spar screwed 10",65.400000000000006,"ΤΕΜ",1,"LP",12,"XPT:8PT6716"]
["XPT:8PT6717","Transverse spar screwed 12",155,"ΤΕΜ",1,"LP",12,"XPT:8PT6717"]
["XPT:8PT6718","Frame profile screwed 0",33.200000000000003,"ΤΕΜ",1,"LP",12,"XPT:8PT6718"]
["XPT:8PT6719","Frame profile screwed 0",39.4,"ΤΕΜ",1,"LP",12,"XPT:8PT6719"]
["XPT:8PT672","Lower front cover for B600",96,"ΤΕΜ",1,"LP",5,"XPT:8PT672"]
["XPT:8PT6720","Frame profile screwed 0",67.599999999999994,"ΤΕΜ",1,"LP",12,"XPT:8PT6720"]
["XPT:8PT6721","Frame profile screwed 1",93.8,"ΤΕΜ",1,"LP",12,"XPT:8PT6721"]
["XPT:8PT6722","Frame profile screwed 1",92.699999999999989,"ΤΕΜ",1,"LP",12,"XPT:8PT6722"]
["XPT:8PT673","Left front cover for B1200",97.6,"ΤΕΜ",1,"LP",5,"XPT:8PT673"]
["XPT:8PT674","Lower front cover for B 1200",90,"ΤΕΜ",1,"LP",5,"XPT:8PT674"]
["XPT:8PT675","Lower front cover for B1200",90,"ΤΕΜ",1,"LP",5,"XPT:8PT675"]
["XPT:8PT676","Right front cover for B1200",146,"ΤΕΜ",1,"LP",5,"XPT:8PT676"]
["XPT:8PT677","Lower front cover for B800",99.699999999999989,"ΤΕΜ",1,"LP",5,"XPT:8PT677"]
["XPT:8PT678","Right compartment cover",132,"ΤΕΜ",1,"LP",5,"XPT:8PT678"]
["XPT:8PT6789","Lever left",7.88,"ΤΕΜ",1,"LP",50,"XPT:8PT6789"]
["XPT:8PT679","Front cover middle support",96.699999999999989,"ΤΕΜ",1,"LP",5,"XPT:8PT679"]
["XPT:8PT681","Cross wiring compartment rear F",79.8,"ΤΕΜ",1,"LP",5,"XPT:8PT681"]
["XPT:8PT682","Partition for B1200",9.7899999999999991,"ΤΕΜ",1,"LP",50,"XPT:8PT682"]
["XPT:8PT683","Cross-wiring compartment rear wall",99.8,"ΤΕΜ",1,"LP",5,"XPT:8PT683"]
["XPT:8PT6836","Mounting plate 300",33.800000000000004,"ΤΕΜ",1,"LP",10,"XPT:8PT6836"]
["XPT:8PT6838","Mounting plate add-on 300",24.200000000000003,"ΤΕΜ",1,"LP",20,"XPT:8PT6838"]
["XPT:8PT684","Cross wiring compartment rear F",65.099999999999994,"ΤΕΜ",1,"LP",5,"XPT:8PT684"]
["XPT:8PT6842","Mounting plate 200",24.700000000000003,"ΤΕΜ",1,"LP",20,"XPT:8PT6842"]
["XPT:8PT685","Center cable way for B1000",12.1,"ΤΕΜ",1,"LP",50,"XPT:8PT685"]
["XPT:8PT6851","Insulating sheet",13.5,"ΤΕΜ",1,"LP",30,"XPT:8PT6851"]
["XPT:8PT6852","Block right OFFD1 UV",76.099999999999994,"ΤΕΜ",1,"LP",5,"XPT:8PT6852"]
["XPT:8PT6853","Block right OFFD1 HV",178,"ΤΕΜ",1,"LP",1,"XPT:8PT6853"]
["XPT:8PT6875","Mounting plate 150",22,"ΤΕΜ",1,"LP",20,"XPT:8PT6875"]
["XPT:8PT6876","Mounting plate add-on 150",14.6,"ΤΕΜ",1,"LP",30,"XPT:8PT6876"]
["XPT:8PT6877","Auxiliary plate 3KL52 300",572,"ΤΕΜ",100,"LP",100,"XPT:8PT6877"]
["XPT:8PT6879","Auxiliary plate 3KL52 200",528,"ΤΕΜ",100,"LP",100,"XPT:8PT6879"]
["XPT:8PT6881","Reinforcement",25.8,"ΤΕΜ",1,"LP",10,"XPT:8PT6881"]
["XPT:8PT6887","Lever right",7.88,"ΤΕΜ",1,"LP",50,"XPT:8PT6887"]
["XPT:8PT6896","Reinforcement",15.799999999999999,"ΤΕΜ",1,"LP",20,"XPT:8PT6896"]
["XPT:8PT6902","Reinforcement 100",13.6,"ΤΕΜ",1,"LP",30,"XPT:8PT6902"]
["XPT:8PT6905","End stop",561,"ΤΕΜ",100,"LP",100,"XPT:8PT6905"]
["XPT:8PT6908","ERI: 551510 support",25.3,"ΤΕΜ",1,"LP",20,"XPT:8PT6908"]
["XPT:8PT6949","Coding part",11.299999999999999,"ΤΕΜ",1,"LP",30,"XPT:8PT6949"]
["XPT:8PT7009","Side wall right 700",67.599999999999994,"ΤΕΜ",1,"LP",5,"XPT:8PT7009"]
["XPT:8PT7010","Side wall left 700",64.3,"ΤΕΜ",1,"LP",5,"XPT:8PT7010"]
["XPT:8PT702","Bottom plate 150x 800",53.6,"ΤΕΜ",1,"LP",10,"XPT:8PT702"]
["XPT:8PT703","Bottom plate 150x 1000",79.8,"ΤΕΜ",1,"LP",5,"XPT:8PT703"]
["XPT:8PT7093","Additional mounting plate 100",73.5,"ΤΕΜ",1,"LP",5,"XPT:8PT7093"]
["XPT:8PT7133","Reinforcement",27.6,"ΤΕΜ",1,"LP",10,"XPT:8PT7133"]
["XPT:8PT7152","Cover compensation field OBE",16.900000000000002,"ΤΕΜ",1,"LP",20,"XPT:8PT7152"]
["XPT:8PT7153","Cover compensation field OBE",19.600000000000001,"ΤΕΜ",1,"LP",20,"XPT:8PT7153"]
["XPT:8PT7169","Bars 4KT8",440,"ΤΕΜ",100,"LP",100,"XPT:8PT7169"]
["XPT:8PT7193","Cover 400 202_5/140 8UC61/62 S",83.8,"ΤΕΜ",1,"LP",5,"XPT:8PT7193"]
["XPT:8PT7194","Cover 300 mm 162.5/80 8UC61/62",75.699999999999989,"ΤΕΜ",1,"LP",5,"XPT:8PT7194"]
["XPT:8PT7195","Cover 300 mm 162.5/115 8UC61/62",75.699999999999989,"ΤΕΜ",1,"LP",5,"XPT:8PT7195"]
["XPT:8PT7196","Cover 500mm 162.5/180 8UC63/66",97.5,"ΤΕΜ",1,"LP",5,"XPT:8PT7196"]
["XPT:8PT7197","Cover 400 162.5/180 8UC63/66 S",83.8,"ΤΕΜ",1,"LP",5,"XPT:8PT7197"]
["XPT:8PT7200","Cover compensation field below",29.2,"ΤΕΜ",1,"LP",10,"XPT:8PT7200"]
["XPT:8PT7228","Door 20X04 right IP54",628,"ΤΕΜ",1,"LP",1,"XPT:8PT7228"]
["XPT:8PT7229","Door 20X06 right IP54",832,"ΤΕΜ",1,"LP",1,"XPT:8PT7229"]
["XPT:8PT7230","Door 20X08 right IP54",1025,"ΤΕΜ",1,"LP",1,"XPT:8PT7230"]
["XPT:8PT7257","Bars 4KT12 3VF6",10.6,"ΤΕΜ",1,"LP",50,"XPT:8PT7257"]
["XPT:8PT7263","Reinforcement",29.2,"ΤΕΜ",1,"LP",10,"XPT:8PT7263"]
["XPT:8PT7272","Reinforcement",27.6,"ΤΕΜ",1,"LP",10,"XPT:8PT7272"]
["XPT:8PT732","Reinforcement connection rail",46.9,"ΤΕΜ",1,"LP",10,"XPT:8PT732"]
["XPT:8PT733","Holder for PE field bar",27.1,"ΤΕΜ",1,"LP",10,"XPT:8PT733"]
["XPT:8PT741","Free cover 25mm",27.6,"ΤΕΜ",1,"LP",10,"XPT:8PT741"]
["XPT:8PT742","Free cover 50mm",31.6,"ΤΕΜ",1,"LP",10,"XPT:8PT742"]
["XPT:8PT743","Free cover 75mm",44.300000000000004,"ΤΕΜ",1,"LP",10,"XPT:8PT743"]
["XPT:8PT744","Free cover 100mm",48,"ΤΕΜ",1,"LP",10,"XPT:8PT744"]
["XPT:8PT7468","Compartment door IP54 H575 W350 left",246,"ΤΕΜ",1,"LP",1,"XPT:8PT7468"]
["XPT:8PT7469","Compartment door H575 W350 RI",144,"ΤΕΜ",1,"LP",1,"XPT:8PT7469"]
["XPT:8PT7470","Compartment door IP54 H575 W350 RI",246,"ΤΕΜ",1,"LP",1,"XPT:8PT7470"]
["XPT:8PT7471","Compartment door H575 W650 LE",256,"ΤΕΜ",1,"LP",1,"XPT:8PT7471"]
["XPT:8PT7472","Compartment door IP54 H575 W650 left",377,"ΤΕΜ",1,"LP",1,"XPT:8PT7472"]
["XPT:8PT7473","Compartment door IP54 H575 W650 RI",392,"ΤΕΜ",1,"LP",1,"XPT:8PT7473"]
["XPT:8PT7475","Cover 600mm 162.5/282 8UC63/66",115,"ΤΕΜ",1,"LP",5,"XPT:8PT7475"]
["XPT:8PT748","Brace H1900",115,"ΤΕΜ",1,"LP",5,"XPT:8PT748"]
["XPT:8PT7620","Spacer 3VF6 3-pole",51,"ΤΕΜ",1,"LP",10,"XPT:8PT7620"]
["XPT:8PT7622","Mounting plate add-on 600",43.6,"ΤΕΜ",1,"LP",10,"XPT:8PT7622"]
["XPT:8PT7640","Compartment door H725 W800 left",450,"ΤΕΜ",1,"LP",1,"XPT:8PT7640"]
["XPT:8PT7641","Compartment door H725 W800 left IP54",605,"ΤΕΜ",1,"LP",1,"XPT:8PT7641"]
["XPT:8PT7642","Door H575 W800 left ventilated",414,"ΤΕΜ",1,"LP",1,"XPT:8PT7642"]
["XPT:8PT7655","Door H575 W800 left ventilated",617,"ΤΕΜ",1,"LP",1,"XPT:8PT7655"]
["XPT:8PT7658","Cover Front 3WN1 W800",74.5,"ΤΕΜ",1,"LP",5,"XPT:8PT7658"]
["XPT:8PT7663","Cover 500mm 162.5/80 8UC61/62",106,"ΤΕΜ",1,"LP",5,"XPT:8PT7663"]
["XPT:8PT7664","Cover 400mm 202_5/80 8UC61/62",83.8,"ΤΕΜ",1,"LP",5,"XPT:8PT7664"]
["XPT:8PT7665","Cover 500mm 202.5/140 8UC61/62",97.5,"ΤΕΜ",1,"LP",5,"XPT:8PT7665"]
["XPT:8PT7666","Cover 600mm 202.5/140 8UC61/62",115,"ΤΕΜ",1,"LP",5,"XPT:8PT7666"]
["XPT:8PT7667","Cover 700mm 162.5/282 8UC63/66",139,"ΤΕΜ",1,"LP",5,"XPT:8PT7667"]
["XPT:8PT7668","Cover 200 mm 162.5/80 8UC61/62",50.6,"ΤΕΜ",1,"LP",10,"XPT:8PT7668"]
["XPT:8PT7669","Cover 400mm 162.5/80 8UC61/62",83.8,"ΤΕΜ",1,"LP",5,"XPT:8PT7669"]
["XPT:8PT7670","Cover 400mm 162.5/180 8UC63/66",83.8,"ΤΕΜ",1,"LP",5,"XPT:8PT7670"]
["XPT:8PT7671","Cover 500mm 162.5/180 8UC63/66",97.5,"ΤΕΜ",1,"LP",5,"XPT:8PT7671"]
["XPT:8PT7672","Cover 600mm 162.5/180 8UC63/66",115,"ΤΕΜ",1,"LP",5,"XPT:8PT7672"]
["XPT:8PT7673","Cover 500mm 162.5/225 8UC63/66",97.5,"ΤΕΜ",1,"LP",5,"XPT:8PT7673"]
["XPT:8PT7674","Cover 600mm 162.5/225 8UC63/66",116,"ΤΕΜ",1,"LP",5,"XPT:8PT7674"]
["XPT:8PT7675","Cover 700mm 162.5/225 8UC63/66",139,"ΤΕΜ",1,"LP",5,"XPT:8PT7675"]
["XPT:8PT7693","Vertical strut 206",16.200000000000003,"ΤΕΜ",1,"LP",20,"XPT:8PT7693"]
["XPT:8PT7694","Vertical strut 1822",132,"ΤΕΜ",1,"LP",5,"XPT:8PT7694"]
["XPT:8PT7695","Holder at the back",6.81,"ΤΕΜ",1,"LP",50,"XPT:8PT7695"]
["XPT:8PT7696","Holder front",16.900000000000002,"ΤΕΜ",1,"LP",20,"XPT:8PT7696"]
["XPT:8PT7697","Holder",10.199999999999999,"ΤΕΜ",1,"LP",50,"XPT:8PT7697"]
["XPT:8PT7698","Horizontal fastening",6.15,"ΤΕΜ",1,"LP",100,"XPT:8PT7698"]
["XPT:8PT7699","Vertical fastening 100",237,"ΤΕΜ",100,"LP",150,"XPT:8PT7699"]
["XPT:8PT7700","Vertical fastening 150",266,"ΤΕΜ",100,"LP",100,"XPT:8PT7700"]
["XPT:8PT7701","Vertical fastening 200",301,"ΤΕΜ",100,"LP",100,"XPT:8PT7701"]
["XPT:8PT7702","Vertical fastening 300",395,"ΤΕΜ",100,"LP",100,"XPT:8PT7702"]
["XPT:8PT7703","Vertical fastening 400",465,"ΤΕΜ",100,"LP",100,"XPT:8PT7703"]
["XPT:8PT7704","Vertical fastening 500",528,"ΤΕΜ",100,"LP",100,"XPT:8PT7704"]
["XPT:8PT7705","Vertical fastening 600",6.15,"ΤΕΜ",1,"LP",100,"XPT:8PT7705"]
["XPT:8PT7706","Vertical fastening 700",6.81,"ΤΕΜ",1,"LP",50,"XPT:8PT7706"]
["XPT:8PT776","Free cover 125mm",51.7,"ΤΕΜ",1,"LP",10,"XPT:8PT776"]
["XPT:8PT777","Free cover 200mm",86,"ΤΕΜ",1,"LP",5,"XPT:8PT777"]
["XPT:8PT778","Free cover 300mm",105,"ΤΕΜ",1,"LP",5,"XPT:8PT778"]
["XPT:8PT7794","Base compartment door H225 left",127,"ΤΕΜ",1,"LP",1,"XPT:8PT7794"]
["XPT:8PT7795","Base compartment door H225 right",127,"ΤΕΜ",1,"LP",1,"XPT:8PT7795"]
["XPT:8PT7796","Base compartment door IP30/40 H225 LEFT",140,"ΤΕΜ",1,"LP",1,"XPT:8PT7796"]
["XPT:8PT7797","Base compartment door IP30/40 H225 RIGHT",140,"ΤΕΜ",1,"LP",1,"XPT:8PT7797"]
["XPT:8PT7802","Base compartment door IP54 H225 left",231,"ΤΕΜ",1,"LP",1,"XPT:8PT7802"]
["XPT:8PT7803","Base compartment door IP54 H225 right",231,"ΤΕΜ",1,"LP",1,"XPT:8PT7803"]
["XPT:8PT7804","Base compartment door IP42 H225 left",298,"ΤΕΜ",1,"LP",1,"XPT:8PT7804"]
["XPT:8PT7805","Base compartment door IP42 H225 right",308,"ΤΕΜ",1,"LP",1,"XPT:8PT7805"]
["XPT:8PT7809","Base compartment door H150 W800 Ventilated",156,"ΤΕΜ",1,"LP",1,"XPT:8PT7809"]
["XPT:8PT7812","Base compartment door IP54 left, right H175",220,"ΤΕΜ",1,"LP",1,"XPT:8PT7812"]
["XPT:8PT7814","Base compartment door IP42 H150W800 RIGHT",318,"ΤΕΜ",1,"LP",1,"XPT:8PT7814"]
["XPT:8PT7818","Base compartment door IP42 H150W800 LEFT",318,"ΤΕΜ",1,"LP",1,"XPT:8PT7818"]
["XPT:8PT7845","Base compartment door H150 W800, not ventilated",138,"ΤΕΜ",1,"LP",1,"XPT:8PT7845"]
["XPT:8PT7857","Spring VD 152B GUTEKUNST",6.15,"ΤΕΜ",1,"LP",50,"XPT:8PT7857"]
["XPT:8PT7860","Cover enclosure",119,"ΤΕΜ",1,"LP",5,"XPT:8PT7860"]
["XPT:8PT7866","Reinforcement",28.200000000000003,"ΤΕΜ",1,"LP",10,"XPT:8PT7866"]
["XPT:8PT7868","Phoenix ST",69.099999999999994,"ΤΕΜ",1,"LP",10,"XPT:8PT7868"]
["XPT:8PT7869","Phoenix BU",44,"ΤΕΜ",1,"LP",10,"XPT:8PT7869"]
["XPT:8PT7870","PHO: 1886333 adapter",18.600000000000001,"ΤΕΜ",1,"LP",20,"XPT:8PT7870"]
["XPT:8PT7871","PHO: 1886142 bus clamp connector",25.3,"ΤΕΜ",1,"LP",10,"XPT:8PT7871"]
["XPT:8PT7872","PHO: 1886139 bus-clamp socket",25.3,"ΤΕΜ",1,"LP",10,"XPT:8PT7872"]
["XPT:8PT7873","PHO: 1886346 D-sub connector",133,"ΤΕΜ",1,"LP",1,"XPT:8PT7873"]
["XPT:8PT8014","Mounting plate 800 LT2",122,"ΤΕΜ",1,"LP",5,"XPT:8PT8014"]
["XPT:8PT8015","Partition mounting plate LT2 800",59.800000000000004,"ΤΕΜ",1,"LP",5,"XPT:8PT8015"]
["XPT:8PT8045","Cover 100 mm 162.5/39 8UC61/62",44.7,"ΤΕΜ",1,"LP",10,"XPT:8PT8045"]
["XPT:8PT8047","Cover 200 mm 162.5/39 8UC61/62",50.6,"ΤΕΜ",1,"LP",10,"XPT:8PT8047"]
["XPT:8PT8092","Control",6.81,"ΤΕΜ",1,"LP",50,"XPT:8PT8092"]
["XPT:8PT8122","Side wall right 150",14.6,"ΤΕΜ",1,"LP",30,"XPT:8PT8122"]
["XPT:8PT8123","Side wall left 150",14.6,"ΤΕΜ",1,"LP",30,"XPT:8PT8123"]
["XPT:8PT8141","Mounting plate",63.5,"ΤΕΜ",1,"LP",5,"XPT:8PT8141"]
["XPT:8PT8148","Cover 1 3VL630 CCS3",78.599999999999994,"ΤΕΜ",1,"LP",5,"XPT:8PT8148"]
["XPT:8PT8149","Mounting plate 375x 600 3VL630 CCS",77.899999999999991,"ΤΕΜ",1,"LP",5,"XPT:8PT8149"]
["XPT:8PT8150","Leaf spring",284,"ΤΕΜ",100,"LP",100,"XPT:8PT8150"]
["XPT:8PT8151","Lever 6",17.400000000000002,"ΤΕΜ",1,"LP",50,"XPT:8PT8151"]
["XPT:8PT8152","Lever 8",7.88,"ΤΕΜ",1,"LP",50,"XPT:8PT8152"]
["XPT:8PT8153","Lever 10",11.299999999999999,"ΤΕΜ",1,"LP",30,"XPT:8PT8153"]
["XPT:8PT8154","Lever 12",21.400000000000002,"ΤΕΜ",1,"LP",20,"XPT:8PT8154"]
["XPT:8PT8297","Mounting plate 275x 600 VL250 CCS3",56.1,"ΤΕΜ",1,"LP",10,"XPT:8PT8297"]
["XPT:8PT8305","Mounting plate 300",34.9,"ΤΕΜ",1,"LP",10,"XPT:8PT8305"]
["XPT:8PT8310","Mounting plate add-on 300",30.900000000000002,"ΤΕΜ",1,"LP",10,"XPT:8PT8310"]
["XPT:8PT8318","Setting ring 10 DIN705",5.62,"ΤΕΜ",1,"LP",200,"XPT:8PT8318"]
["XPT:8PT8319","Setting ring 12 DIN705",6.15,"ΤΕΜ",1,"LP",100,"XPT:8PT8319"]
["XPT:8PT8342","Mounting plate 375x 600 3VF6 CCS3",77.899999999999991,"ΤΕΜ",1,"LP",5,"XPT:8PT8342"]
["XPT:8PT8344","Cover 1 3VF6 CCS3",78.3,"ΤΕΜ",1,"LP",5,"XPT:8PT8344"]
["XPT:8PT8345","Mounting plate 375x 600 3VF6 3-pole",77.899999999999991,"ΤΕΜ",1,"LP",5,"XPT:8PT8345"]
["XPT:8PT8347","Cover 1 3VF6 3-pole CCS3",32.6,"ΤΕΜ",1,"LP",10,"XPT:8PT8347"]
["XPT:8PT8348","Cover 2 3VF6 3-pole CCS3",27.6,"ΤΕΜ",1,"LP",10,"XPT:8PT8348"]
["XPT:8PT8350","Locking plate",295,"ΤΕΜ",100,"LP",100,"XPT:8PT8350"]
["XPT:8PT8353","Plastic rivet",232,"ΤΕΜ",1000,"LP",1000,"XPT:8PT8353"]
["XPT:8PT8354","Bellows",6.15,"ΤΕΜ",1,"LP",50,"XPT:8PT8354"]
["XPT:8PT8362","Reinforcement",27.6,"ΤΕΜ",1,"LP",10,"XPT:8PT8362"]
["XPT:8PT8371","Rear panel W400 H400 unventilated",72.599999999999994,"ΤΕΜ",1,"LP",5,"XPT:8PT8371"]
["XPT:8PT8382","Frame profile screwed B700",108,"ΤΕΜ",1,"LP",2,"XPT:8PT8382"]
["XPT:8PT8383","Frame profile T700",76.099999999999994,"ΤΕΜ",1,"LP",2,"XPT:8PT8383"]
["XPT:8PT8384","Mounting bracket top corner",33.200000000000003,"ΤΕΜ",1,"LP",10,"XPT:8PT8384"]
["XPT:8PT8385","Corner plate top",36.6,"ΤΕΜ",1,"LP",10,"XPT:8PT8385"]
["XPT:8PT8386","Bottom plate corner cupboard 600",69.099999999999994,"ΤΕΜ",1,"LP",5,"XPT:8PT8386"]
["XPT:8PT8387","Mounting bracket bottom corner",33.200000000000003,"ΤΕΜ",1,"LP",10,"XPT:8PT8387"]
["XPT:8PT8388","Frame profile corner",298,"ΤΕΜ",1,"LP",1,"XPT:8PT8388"]
["XPT:8PT8389","Frame profile corner",226,"ΤΕΜ",1,"LP",1,"XPT:8PT8389"]
["XPT:8PT8390","Bottom plate corner cupboard",34.9,"ΤΕΜ",1,"LP",10,"XPT:8PT8390"]
["XPT:8PT8413","Rear panel W400 H400 IP30, GEPUL",85.699999999999989,"ΤΕΜ",1,"LP",5,"XPT:8PT8413"]
["XPT:8PT8453","Reinforcement",27.6,"ΤΕΜ",1,"LP",10,"XPT:8PT8453"]
["XPT:8PT8464","Mounting tool for output contacts",9447,"ΤΕΜ",1,"LP",1,"XPT:8PT8464"]
["XPT:8PT8465","Mounting tool for input",9447,"ΤΕΜ",1,"LP",1,"XPT:8PT8465"]
["XPT:8PT8466","Rear panel W400 H400 IP42GEPULVE",96.8,"ΤΕΜ",1,"LP",5,"XPT:8PT8466"]
["XPT:8PT8495","Reinforcement",27.1,"ΤΕΜ",1,"LP",10,"XPT:8PT8495"]
["XPT:8PT8498","Insulation strips",14.6,"ΤΕΜ",1,"LP",20,"XPT:8PT8498"]
["XPT:8PT8528","Latching sheet",42.1,"ΤΕΜ",1,"LP",10,"XPT:8PT8528"]
["XPT:8PT8531","Cover 200 mm 162.5/100 8UC61/62",71.599999999999994,"ΤΕΜ",1,"LP",5,"XPT:8PT8531"]
["XPT:8PT8532","Cover 300 mm 162.5/100 8UC61/62",81.199999999999989,"ΤΕΜ",1,"LP",5,"XPT:8PT8532"]
["XPT:8PT8533","Cover 300 mm 202.5/115 8UC61/62",81.199999999999989,"ΤΕΜ",1,"LP",5,"XPT:8PT8533"]
["XPT:8PT8534","Cover 400mm 202.5/115 8UC61/62",88.2,"ΤΕΜ",1,"LP",5,"XPT:8PT8534"]
["XPT:8PT9060","Mounting plate add-on 200",53.2,"ΤΕΜ",1,"LP",5,"XPT:8PT9060"]
["XPT:8PT9120","Mounting bracket for bar",20.900000000000002,"ΤΕΜ",1,"LP",20,"XPT:8PT9120"]
["XPT:8PT9121","Clamping plate corner cubicle HV",16.3,"ΤΕΜ",1,"LP",20,"XPT:8PT9121"]
["XPT:8PT9122","Clamping plate corner cubicle 600",84.899999999999991,"ΤΕΜ",1,"LP",5,"XPT:8PT9122"]
["XPT:8PT9123","Clamping plate corner cubicle 800",103,"ΤΕΜ",1,"LP",5,"XPT:8PT9123"]
["XPT:8PT9131","Frame profile screwed B900",109,"ΤΕΜ",1,"LP",2,"XPT:8PT9131"]
["XPT:8PT9132","Frame profile T700",75.699999999999989,"ΤΕΜ",1,"LP",2,"XPT:8PT9132"]
["XPT:8PT9140","Rear wall 700 unventilated",388,"ΤΕΜ",1,"LP",1,"XPT:8PT9140"]
["XPT:8PT9141","Rear wall 700 unventilated IP30",425,"ΤΕΜ",1,"LP",1,"XPT:8PT9141"]
["XPT:8PT9142","Rear wall 700 unventilated IP42",429,"ΤΕΜ",1,"LP",1,"XPT:8PT9142"]
["XPT:8PT9143","Rear wall 900 unventilated",392,"ΤΕΜ",1,"LP",1,"XPT:8PT9143"]
["XPT:8PT9144","Rear wall 900 ventilated IP30",432,"ΤΕΜ",1,"LP",1,"XPT:8PT9144"]
["XPT:8PT9145","Rear wall 900 ventilated IP42",462,"ΤΕΜ",1,"LP",1,"XPT:8PT9145"]
["XPT:8PT9146","Side wall 700",367,"ΤΕΜ",1,"LP",1,"XPT:8PT9146"]
["XPT:8PT9147","Side wall 900",384,"ΤΕΜ",1,"LP",1,"XPT:8PT9147"]
["XPT:8PT9148","Top plate corner cubicle 600",155,"ΤΕΜ",1,"LP",1,"XPT:8PT9148"]
["XPT:8PT9149","Top plate corner cubicle 800",195,"ΤΕΜ",1,"LP",1,"XPT:8PT9149"]
["XPT:8PT9150","Bottom plate 1 corner cupboard 800",117,"ΤΕΜ",1,"LP",5,"XPT:8PT9150"]
["XPT:8PT9151","Bottom plate 2 corner cupboard 800",65.699999999999989,"ΤΕΜ",1,"LP",5,"XPT:8PT9151"]
["XPT:8PT9170","Label interlock",175,"ΤΕΜ",100,"LP",250,"XPT:8PT9170"]
["XPT:8PT9183","Support for vertical bar",33.800000000000004,"ΤΕΜ",1,"LP",10,"XPT:8PT9183"]
["XPT:8PT9188","Grounding cable Horstmann: 61-0103-",345,"ΤΕΜ",1,"LP",1,"XPT:8PT9188"]
["XPT:8PT9240","Support VL630",39.5,"ΤΕΜ",1,"LP",10,"XPT:8PT9240"]
["XPT:8PT9241","Cover VL630 4-pole",135,"ΤΕΜ",1,"LP",5,"XPT:8PT9241"]
["XPT:8PT9261","Mounting plate 275x 600 3KL55, 3KL57 C",55.800000000000004,"ΤΕΜ",1,"LP",10,"XPT:8PT9261"]
["XPT:8PT9262","Cover 1 3KL57 CCS3",40.6,"ΤΕΜ",1,"LP",10,"XPT:8PT9262"]
["XPT:8PT9263","Cover 2 3KL57/55 CCS3",28.200000000000003,"ΤΕΜ",1,"LP",10,"XPT:8PT9263"]
["XPT:8PT9270","Cover VL630 3-pole",109,"ΤΕΜ",1,"LP",5,"XPT:8PT9270"]
["XPT:8PT9271","Mounting plate 375",51.7,"ΤΕΜ",1,"LP",10,"XPT:8PT9271"]
["XPT:8PT9276","Cover 1 3KL55 CCS3",40.6,"ΤΕΜ",1,"LP",10,"XPT:8PT9276"]
["XPT:8PT9283","Mounting plate 200",33.200000000000003,"ΤΕΜ",1,"LP",10,"XPT:8PT9283"]
["XPT:8PT9284","Mounting plate 200",22.5,"ΤΕΜ",1,"LP",20,"XPT:8PT9284"]
["XPT:8PT9299","Support 3NP5460",31.6,"ΤΕΜ",1,"LP",10,"XPT:8PT9299"]
["XPT:8PT9300","Cover 3NP5460",135,"ΤΕΜ",1,"LP",5,"XPT:8PT9300"]
["XPT:8PT9321","Mounting plate 475x 600 3KL61 CCS3",87.899999999999991,"ΤΕΜ",1,"LP",5,"XPT:8PT9321"]
["XPT:8PT9322","Cover 1 3KL61 CCS3",39.9,"ΤΕΜ",1,"LP",5,"XPT:8PT9322"]
["XPT:8PT9323","Cover 2 3KL61 CCS3",68.3,"ΤΕΜ",1,"LP",5,"XPT:8PT9323"]
["XPT:8PT9324","Spacer 3KL61 CCS3",26.5,"ΤΕΜ",1,"LP",10,"XPT:8PT9324"]
["XPT:8PT9362","Cover 3VF6 4-pole",135,"ΤΕΜ",1,"LP",5,"XPT:8PT9362"]
["XPT:8PT9363","Support 3VF6",39.5,"ΤΕΜ",1,"LP",10,"XPT:8PT9363"]
["XPT:8PT9364","Cover 3VF6 3-pole",135,"ΤΕΜ",1,"LP",5,"XPT:8PT9364"]
["XPT:8PT9370","Support 3NP5360",31.6,"ΤΕΜ",1,"LP",10,"XPT:8PT9370"]
["XPT:8PT9371","Support 3VF5",42.1,"ΤΕΜ",1,"LP",10,"XPT:8PT9371"]
["XPT:8PT9377","Mounting plate 275x 600 3KL53 CCS3",55.800000000000004,"ΤΕΜ",1,"LP",10,"XPT:8PT9377"]
["XPT:8PT9378","Cover 1 3KL53 CCS3",41,"ΤΕΜ",1,"LP",10,"XPT:8PT9378"]
["XPT:8PT9379","Cover 2 3KL53 CCS3",25.8,"ΤΕΜ",1,"LP",10,"XPT:8PT9379"]
["XPT:8PT9387","Cover 1 3KL53 4P CCS3",41,"ΤΕΜ",1,"LP",10,"XPT:8PT9387"]
["XPT:8PT9414","Side wall 100 corner cabinet",122,"ΤΕΜ",1,"LP",5,"XPT:8PT9414"]
["XPT:8PT9415","Side wall 200 corner cabinet",212,"ΤΕΜ",1,"LP",5,"XPT:8PT9415"]
["XPT:8PT9416","Mounting bracket side wall E",14.6,"ΤΕΜ",1,"LP",30,"XPT:8PT9416"]
["XPT:8PT9421","Mounting plate 375x 600 SENTLF CCS",73.399999999999991,"ΤΕΜ",1,"LP",5,"XPT:8PT9421"]
["XPT:8PT9422","Mounting plate 375x 600 3NP54 CCS3",78.599999999999994,"ΤΕΜ",1,"LP",5,"XPT:8PT9422"]
["XPT:8PT9453","Mounting plate 375x 600 3KL57 4P C",78.3,"ΤΕΜ",1,"LP",5,"XPT:8PT9453"]
["XPT:8PT9454","Cover 1 3KL57 4P CCS3",41.4,"ΤΕΜ",1,"LP",10,"XPT:8PT9454"]
["XPT:8PT9455","Cover 2 3KL57 4P CCS3",39.9,"ΤΕΜ",1,"LP",10,"XPT:8PT9455"]
["XPT:8PT9456","Cover 1 3KL55 4P CCS3",41.4,"ΤΕΜ",1,"LP",10,"XPT:8PT9456"]
["XPT:8PT9473","Transport stiffening",31.6,"ΤΕΜ",1,"LP",10,"XPT:8PT9473"]
["XPT:8PT9478","Mounting plate for VL630",54.300000000000004,"ΤΕΜ",1,"LP",10,"XPT:8PT9478"]
["XPT:8PT9487","Mounting plate 475x 600 3KL61 4P C",87.5,"ΤΕΜ",1,"LP",5,"XPT:8PT9487"]
["XPT:8PT9488","Cover 1 3KL61 4P CCS3",42.5,"ΤΕΜ",1,"LP",10,"XPT:8PT9488"]
["XPT:8PT9489","Cover 2 3KL61 4P CCS3",76.099999999999994,"ΤΕΜ",1,"LP",5,"XPT:8PT9489"]
["XPT:8PT9504","Mounting plate 175x 600 VL160 3P C",43.6,"ΤΕΜ",1,"LP",10,"XPT:8PT9504"]
["XPT:8PT9505","Cover 1 VL160 3P CCS3",38.4,"ΤΕΜ",1,"LP",10,"XPT:8PT9505"]
["XPT:8PT9506","Cover 2 VL160 3P CCS3",29.2,"ΤΕΜ",1,"LP",10,"XPT:8PT9506"]
["XPT:8PT9536","Mounting plate 175x 600 VL160X 3P",43.6,"ΤΕΜ",1,"LP",10,"XPT:8PT9536"]
["XPT:8PT9537","Mounting plate 275x 600 VL160 4P C",56.9,"ΤΕΜ",1,"LP",5,"XPT:8PT9537"]
["XPT:8PT955","Bracket for transport unit field width 600",99.699999999999989,"ΤΕΜ",1,"LP",2,"XPT:8PT955"]
["XPT:8PT956","Bracket for transport unit field width 800",158,"ΤΕΜ",1,"LP",2,"XPT:8PT956"]
["XPT:8PT9566","Cover 3KL55, 3KL57 3-pole OFF1",105,"ΤΕΜ",1,"LP",5,"XPT:8PT9566"]
["XPT:8PT9567","Mounting plate 3KL55, 3KL57 OFF1",15.799999999999999,"ΤΕΜ",1,"LP",20,"XPT:8PT9567"]
["XPT:8PT9568","Cover 3KL55, 3KL57 4-pol. OFF1",125,"ΤΕΜ",1,"LP",5,"XPT:8PT9568"]
["XPT:8PT957","Bracket for transport unit field width 1000",103,"ΤΕΜ",1,"LP",2,"XPT:8PT957"]
["XPT:8PT958","Bracket for transport unit field width 1200",161,"ΤΕΜ",1,"LP",2,"XPT:8PT958"]
["XPT:8PT9607","Spacer VL630 CCS3",31.6,"ΤΕΜ",1,"LP",10,"XPT:8PT9607"]
["XPT:8PT9617","Short circuit support front",10.199999999999999,"ΤΕΜ",1,"LP",50,"XPT:8PT9617"]
["XPT:8PT9624","Fuse tongs size: 00",447,"ΤΕΜ",1,"LP",1,"XPT:8PT9624"]
["XPT:8PT9625","Fuse tongs size: 1-3",447,"ΤΕΜ",1,"LP",1,"XPT:8PT9625"]
["XPT:8PT9626","Test adapter plug-in connection",6864,"ΤΕΜ",1,"LP",1,"XPT:8PT9626"]
["XPT:8PT9627","Test adapter /plug-in withdrawable connection",8856,"ΤΕΜ",1,"LP",1,"XPT:8PT9627"]
["XPT:8PT963","Vertical busbar holder",105,"ΤΕΜ",1,"LP",5,"XPT:8PT963"]
["XPT:8PT964","Partition,",155,"ΤΕΜ",1,"LP",1,"XPT:8PT964"]
["XPT:8PT965","Partition,",213,"ΤΕΜ",1,"LP",1,"XPT:8PT965"]
["XPT:8PT9655","Cover 3KL50/52/53 4POLOFF",78.3,"ΤΕΜ",1,"LP",5,"XPT:8PT9655"]
["XPT:8PT966","Partition plate support bracket",221,"ΤΕΜ",100,"LP",100,"XPT:8PT966"]
["XPT:8PT9663","Support L400",39.5,"ΤΕΜ",1,"LP",10,"XPT:8PT9663"]
["XPT:8PT9664","Cover VL400 4-pole",161,"ΤΕΜ",1,"LP",5,"XPT:8PT9664"]
["XPT:8PT9665","Cover VL400 3-pole",140,"ΤΕΜ",1,"LP",5,"XPT:8PT9665"]
["XPT:8PT9667","Latch plate",524,"ΤΕΜ",100,"LP",100,"XPT:8PT9667"]
["XPT:8PT967","Partition wall T 600",170,"ΤΕΜ",1,"LP",1,"XPT:8PT967"]
["XPT:8PT9674","Cover 3KL50 CCS3",38.4,"ΤΕΜ",1,"LP",10,"XPT:8PT9674"]
["XPT:8PT9675","Mounting plate 175x 600 3KL50 3P C",43.6,"ΤΕΜ",1,"LP",10,"XPT:8PT9675"]
["XPT:8PT9676","Mounting plate 3KL52 50 CCS3",55.4,"ΤΕΜ",1,"LP",10,"XPT:8PT9676"]
["XPT:8PT9677","Cover 3KL52 50 CCS3",76.099999999999994,"ΤΕΜ",1,"LP",5,"XPT:8PT9677"]
["XPT:8PT968","Partition wall T 800",305,"ΤΕΜ",1,"LP",1,"XPT:8PT968"]
["XPT:8PT9683","Handle",14.1,"ΤΕΜ",1,"LP",30,"XPT:8PT9683"]
["XPT:8PT969","Partition wall T 1000",307,"ΤΕΜ",1,"LP",1,"XPT:8PT969"]
["XPT:8PT9698","Mounting plate 125 mm",20.900000000000002,"ΤΕΜ",1,"LP",20,"XPT:8PT9698"]
["XPT:8PT9704","Holder",11.299999999999999,"ΤΕΜ",1,"LP",30,"XPT:8PT9704"]
["XPT:8PT9710","Support plate for 3UA66",19.200000000000003,"ΤΕΜ",1,"LP",20,"XPT:8PT9710"]
["XPT:8PT9711","Mounting plate 600",44,"ΤΕΜ",1,"LP",10,"XPT:8PT9711"]
["XPT:8PT9712","Mounting plate 600",48,"ΤΕΜ",1,"LP",10,"XPT:8PT9712"]
["XPT:8PT9735","Mounting plate 175 mm",21.400000000000002,"ΤΕΜ",1,"LP",20,"XPT:8PT9735"]
["XPT:8PT9761","Mounting plate 75 mm",16.3,"ΤΕΜ",1,"LP",20,"XPT:8PT9761"]
["XPT:8PT9774","Mounting plate H300 OFPM",50.2,"ΤΕΜ",1,"LP",10,"XPT:8PT9774"]
["XPT:8PT980","Brace L 740",33.800000000000004,"ΤΕΜ",1,"LP",10,"XPT:8PT980"]
["XPT:8PT981","Brace L 940",48,"ΤΕΜ",1,"LP",10,"XPT:8PT981"]
["XPT:8PT9818","Compartment bottom 3WL W600",63.5,"ΤΕΜ",1,"LP",5,"XPT:8PT9818"]
["XPT:8PT982","Front plate 400",17.900000000000002,"ΤΕΜ",1,"LP",20,"XPT:8PT982"]
["XPT:8PT983","Front plate 600",23.1,"ΤΕΜ",1,"LP",20,"XPT:8PT983"]
["XPT:8PT984","Device holder 1675x 1000 MPC",234,"ΤΕΜ",1,"LP",1,"XPT:8PT984"]
["XPT:8PT985","Door IP54 H300 B600",237,"ΤΕΜ",1,"LP",1,"XPT:8PT985"]
["XPT:8PT986","Door IP54 H300 B800",270,"ΤΕΜ",1,"LP",1,"XPT:8PT986"]
["XPT:8PT9864","Vertical busbar support",64.3,"ΤΕΜ",1,"LP",5,"XPT:8PT9864"]
["XPT:8PT9865","Busbar support W400",35.4,"ΤΕΜ",1,"LP",10,"XPT:8PT9865"]
["XPT:8PT9866","Compartment bottom 3WL BG1 400",52.4,"ΤΕΜ",1,"LP",10,"XPT:8PT9866"]
["XPT:8PT9867","Mounting plate 400",63.5,"ΤΕΜ",1,"LP",5,"XPT:8PT9867"]
["XPT:8PT987","Door IP54 H300 B1000",273,"ΤΕΜ",1,"LP",1,"XPT:8PT987"]
["XPT:8PT9871","Support horizontal 400",18.600000000000001,"ΤΕΜ",1,"LP",20,"XPT:8PT9871"]
["XPT:8PT988","Door IP42 H1900 B400 LEFT",580,"ΤΕΜ",1,"LP",1,"XPT:8PT988"]
["XPT:8PT989","Door IP42 H2200 B400 LEFT",584,"ΤΕΜ",1,"LP",1,"XPT:8PT989"]
["XPT:8PT9894","Busbar support",85.3,"ΤΕΜ",1,"LP",5,"XPT:8PT9894"]
["XPT:8PT9895","Insulating mat",75.699999999999989,"ΤΕΜ",1,"LP",5,"XPT:8PT9895"]
["XPT:8PT990","Door IP42 H1900 B600 LEFT",731,"ΤΕΜ",1,"LP",1,"XPT:8PT990"]
["XPT:8PT991","Door IP42 H2200 B600 LEFT",761,"ΤΕΜ",1,"LP",1,"XPT:8PT991"]
["XPT:8PT9913","Standard 300 4KT12_VL400",521,"ΤΕΜ",100,"LP",100,"XPT:8PT9913"]
["XPT:8PT9915","Bolt 4KT12 VL400",7.88,"ΤΕΜ",1,"LP",50,"XPT:8PT9915"]
["XPT:8PT992","Door IP42 H1900 B800 LEFT",812,"ΤΕΜ",1,"LP",1,"XPT:8PT992"]
["XPT:8PT993","Door IP42 H2200 B800 LEFY",827,"ΤΕΜ",1,"LP",1,"XPT:8PT993"]
["XPT:8PT994","Door IP42 H2200 B1000 LEFT",941,"ΤΕΜ",1,"LP",1,"XPT:8PT994"]
["XPT:8PT9946","Cover 300 mm 165_5/100 8UC61",77.5,"ΤΕΜ",1,"LP",5,"XPT:8PT9946"]
["XPT:8PT9948","Cover 400 mm 162_5/100 8UC61",78.3,"ΤΕΜ",1,"LP",5,"XPT:8PT9948"]
["XPT:8PT9949","Compartment door W800XH400 MPC",197,"ΤΕΜ",1,"LP",1,"XPT:8PT9949"]
["XPT:8PT995","Door IP42 H1900 B400 RIGHT",580,"ΤΕΜ",1,"LP",1,"XPT:8PT995"]
["XPT:8PT9950","Compartment door W800XH400 IP54",310,"ΤΕΜ",1,"LP",1,"XPT:8PT9950"]
["XPT:8PT996","Door IP42 H2200 B400 RIGHT",584,"ΤΕΜ",1,"LP",1,"XPT:8PT996"]
["XPT:8PT997","Door IP42 H1900 B600 RIGHT",724,"ΤΕΜ",1,"LP",1,"XPT:8PT997"]
["XPT:8PT9970","Connection bar reinforcement W4",49.9,"ΤΕΜ",1,"LP",10,"XPT:8PT9970"]
["XPT:8PT998","Door IP42 H2200 B600 RIGHT",757,"ΤΕΜ",1,"LP",1,"XPT:8PT998"]
["XPT:8PT999","Door IP42 H1900 B800 RIGHT",812,"ΤΕΜ",1,"LP",1,"XPT:8PT999"]
["XPT:8PT9999","Partition 600",51,"ΤΕΜ",1,"LP",10,"XPT:8PT9999"]

{"sheet":"Sheet1","index":1,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["PA","PMD Data available"]
[""]
["VF","Sales Release"]
[""]
["LF","Delivery Release"]
[""]
["AE","Phase Out Announce"]
[""]
["TS","Prod. Cancellation"]
[""]
["MH","Prod. Discont."]
[""]
["AK","End Prod.Lifecycl."]