{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Price List 2020-2021","Sheet1"],"not_rendered":{"charts":0,"images":4,"macros":1,"external_links":0,"defined_names":3,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Price List 2020-2021","index":0,"n_rows":195097,"n_cols":14,"rows_kept":4500,"cut":true,"hidden":false,"merged":[[0,1,0,2],[0,3,0,6],[1,0,1,6],[2,2,2,6],[2,0,2,1]],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
[null,"Siemens Digital Industries\nΤιμοκατάλογος Προϊόντων Βιομηχανίας 2021-2022",null,"Ισχύει από την 01.10.2021 και καταργεί κάθε προηγούμενο. Οι τιμές και τα τεχνικά χαρακτηριστικά των υλικών υπόκεινται σε οποιαδήποτε αλλαγή χωρίς προηγούμενη ειδοποίηση και δεν περιλαμβάνουν ΦΠΑ. "]
["Περιλαμβάνει τις παρακάτω κατηγορίες υλικών:"]
["Βιομηχανικός αυτοματισμός Simatic και Υλικά Δικτύου (Simatic)\nΒιομηχανικός αυτοματισμός Simatic S71200 (S7-1200)\nLOGO!, τροφοδοτικά LOGO! Power (LOGO!)\nΚινητήρες Χαμηλής τάσης AC (LVM) \n",null,"Ηλεκτρολογικό Υλικό Χαμηλής Τάσης (LP) \nΡυθμιστές στροφών και συστήματα ελέγχου κίνησης  Motion control (MC)\nΒιομηχανικό υλικό χαμηλής τάσης (CP)\nΌργανα Μέτρησης Πεδίου (PI1, PI2, PI3)"]
["Αναζήτηση υλικού","Αναζήτηση με:"]
["Κωδικός","Περιγραφή","Τιμή καταλόγου (€)","Μον. Μέτρησης","Ποσ. μονάδας μέτρησης","Κατηγορία υλικού","Ελάχιστη ποσότητα παραγγελίας",null,null,null,"Βάρος","Μονάδα βάρους","UPC Code","EAN Code"]
["1FK2102-0AG00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D8x25 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1090,"ΤΕΜ",1,"MC",1,"1FK21020AG000MA0"]
["1FK2102-0AG00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D8x25 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",769,"ΤΕΜ",1,"MC",1,"1FK21020AG000SA0"]
["1FK2102-0AG00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D8x25mm with fitted key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1090,"ΤΕΜ",1,"MC",1,"1FK21020AG001MA0"]
["1FK2102-0AG00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D8x25mm with fitted key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",769,"ΤΕΜ",1,"MC",1,"1FK21020AG001SA0"]
["1FK2102-0AG01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D8x25 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1179,"ΤΕΜ",1,"MC",1,"1FK21020AG010MA0"]
["1FK2102-0AG01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D8x25 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",858,"ΤΕΜ",1,"MC",1,"1FK21020AG010SA0"]
["1FK2102-0AG01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D8x25mm with fitted key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1179,"ΤΕΜ",1,"MC",1,"1FK21020AG011MA0"]
["1FK2102-0AG01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D8x25mm with fitted key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",858,"ΤΕΜ",1,"MC",1,"1FK21020AG011SA0"]
["1FK2102-0AG10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D8x25 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1304,"ΤΕΜ",1,"MC",1,"1FK21020AG100MA0"]
["1FK2102-0AG10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D8x25 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",983,"ΤΕΜ",1,"MC",1,"1FK21020AG100SA0"]
["1FK2102-0AG10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D8x25mm with fitted key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1304,"ΤΕΜ",1,"MC",1,"1FK21020AG101MA0"]
["1FK2102-0AG10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D8x25mm with fitted key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",983,"ΤΕΜ",1,"MC",1,"1FK21020AG101SA0"]
["1FK2102-0AG11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D8x25 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1394,"ΤΕΜ",1,"MC",1,"1FK21020AG110MA0"]
["1FK2102-0AG11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D8x25 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1073,"ΤΕΜ",1,"MC",1,"1FK21020AG110SA0"]
["1FK2102-0AG11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D8x25mm with fitted key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1394,"ΤΕΜ",1,"MC",1,"1FK21020AG111MA0"]
["1FK2102-0AG11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.16 Nm; PN = 0.05 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D8x25mm with fitted key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1073,"ΤΕΜ",1,"MC",1,"1FK21020AG111SA0"]
["1FK2102-1AG00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D8x25 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1111,"ΤΕΜ",1,"MC",1,"1FK21021AG000MA0"]
["1FK2102-1AG00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D8x25 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",790,"ΤΕΜ",1,"MC",1,"1FK21021AG000SA0"]
["1FK2102-1AG00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D8x25mm with fitted key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1111,"ΤΕΜ",1,"MC",1,"1FK21021AG001MA0"]
["1FK2102-1AG00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D8x25mm with fitted key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",790,"ΤΕΜ",1,"MC",1,"1FK21021AG001SA0"]
["1FK2102-1AG01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D8x25 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1201,"ΤΕΜ",1,"MC",1,"1FK21021AG010MA0"]
["1FK2102-1AG01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D8x25 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",880,"ΤΕΜ",1,"MC",1,"1FK21021AG010SA0"]
["1FK2102-1AG01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D8x25mm with fitted key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1201,"ΤΕΜ",1,"MC",1,"1FK21021AG011MA0"]
["1FK2102-1AG01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D8x25mm with fitted key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",880,"ΤΕΜ",1,"MC",1,"1FK21021AG011SA0"]
["1FK2102-1AG10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D8x25 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1325,"ΤΕΜ",1,"MC",1,"1FK21021AG100MA0"]
["1FK2102-1AG10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D8x25 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1004,"ΤΕΜ",1,"MC",1,"1FK21021AG100SA0"]
["1FK2102-1AG10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D8x25mm with fitted key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1325,"ΤΕΜ",1,"MC",1,"1FK21021AG101MA0"]
["1FK2102-1AG10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D8x25mm with fitted key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1004,"ΤΕΜ",1,"MC",1,"1FK21021AG101SA0"]
["1FK2102-1AG11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D8x25 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1415,"ΤΕΜ",1,"MC",1,"1FK21021AG110MA0"]
["1FK2102-1AG11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D8x25 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1094,"ΤΕΜ",1,"MC",1,"1FK21021AG110SA0"]
["1FK2102-1AG11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D8x25mm with fitted key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1415,"ΤΕΜ",1,"MC",1,"1FK21021AG111MA0"]
["1FK2102-1AG11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.32 Nm; PN = 0.1 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D8x25mm with fitted key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1094,"ΤΕΜ",1,"MC",1,"1FK21021AG111SA0"]
["1FK2103-2AG00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1175,"ΤΕΜ",1,"MC",1,"1FK21032AG000MA0"]
["1FK2103-2AG00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",854,"ΤΕΜ",1,"MC",1,"1FK21032AG000SA0"]
["1FK2103-2AG00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1175,"ΤΕΜ",1,"MC",1,"1FK21032AG001MA0"]
["1FK2103-2AG00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",854,"ΤΕΜ",1,"MC",1,"1FK21032AG001SA0"]
["1FK2103-2AG00-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1175,"ΤΕΜ",1,"MC",1,"1FK21032AG002MA0"]
["1FK2103-2AG00-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",854,"ΤΕΜ",1,"MC",1,"1FK21032AG002SA0"]
["1FK2103-2AG01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1265,"ΤΕΜ",1,"MC",1,"1FK21032AG010MA0"]
["1FK2103-2AG01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",944,"ΤΕΜ",1,"MC",1,"1FK21032AG010SA0"]
["1FK2103-2AG01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1265,"ΤΕΜ",1,"MC",1,"1FK21032AG011MA0"]
["1FK2103-2AG01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",944,"ΤΕΜ",1,"MC",1,"1FK21032AG011SA0"]
["1FK2103-2AG01-2MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M12, rotatable; .",1265,"ΤΕΜ",1,"MC",1,"1FK21032AG012MA0"]
["1FK2103-2AG01-2SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M12, rotatable; .",944,"ΤΕΜ",1,"MC",1,"1FK21032AG012SA0"]
["1FK2103-2AG10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1432,"ΤΕΜ",1,"MC",1,"1FK21032AG100MA0"]
["1FK2103-2AG10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1111,"ΤΕΜ",1,"MC",1,"1FK21032AG100SA0"]
["1FK2103-2AG10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1432,"ΤΕΜ",1,"MC",1,"1FK21032AG101MA0"]
["1FK2103-2AG10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1111,"ΤΕΜ",1,"MC",1,"1FK21032AG101SA0"]
["1FK2103-2AG10-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1432,"ΤΕΜ",1,"MC",1,"1FK21032AG102MA0"]
["1FK2103-2AG10-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1111,"ΤΕΜ",1,"MC",1,"1FK21032AG102SA0"]
["1FK2103-2AG11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1522,"ΤΕΜ",1,"MC",1,"1FK21032AG110MA0"]
["1FK2103-2AG11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1201,"ΤΕΜ",1,"MC",1,"1FK21032AG110SA0"]
["1FK2103-2AG11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1522,"ΤΕΜ",1,"MC",1,"1FK21032AG111MA0"]
["1FK2103-2AG11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1201,"ΤΕΜ",1,"MC",1,"1FK21032AG111SA0"]
["1FK2103-2AG11-2MA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M12, rotatable; .",1522,"ΤΕΜ",1,"MC",1,"1FK21032AG112MA0"]
["1FK2103-2AG11-2SA0","SIMOTICS S-1FK2 HD servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M12, rotatable; .",1201,"ΤΕΜ",1,"MC",1,"1FK21032AG112SA0"]
["1FK2103-4AG00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1303,"ΤΕΜ",1,"MC",1,"1FK21034AG000MA0"]
["1FK2103-4AG00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",982,"ΤΕΜ",1,"MC",1,"1FK21034AG000SA0"]
["1FK2103-4AG00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1303,"ΤΕΜ",1,"MC",1,"1FK21034AG001MA0"]
["1FK2103-4AG00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",982,"ΤΕΜ",1,"MC",1,"1FK21034AG001SA0"]
["1FK2103-4AG00-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1303,"ΤΕΜ",1,"MC",1,"1FK21034AG002MA0"]
["1FK2103-4AG00-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",982,"ΤΕΜ",1,"MC",1,"1FK21034AG002SA0"]
["1FK2103-4AG01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1393,"ΤΕΜ",1,"MC",1,"1FK21034AG010MA0"]
["1FK2103-4AG01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1072,"ΤΕΜ",1,"MC",1,"1FK21034AG010SA0"]
["1FK2103-4AG01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1393,"ΤΕΜ",1,"MC",1,"1FK21034AG011MA0"]
["1FK2103-4AG01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1072,"ΤΕΜ",1,"MC",1,"1FK21034AG011SA0"]
["1FK2103-4AG01-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M12, rotatable; .",1393,"ΤΕΜ",1,"MC",1,"1FK21034AG012MA0"]
["1FK2103-4AG01-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M12, rotatable; .",1072,"ΤΕΜ",1,"MC",1,"1FK21034AG012SA0"]
["1FK2103-4AG10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1560,"ΤΕΜ",1,"MC",1,"1FK21034AG100MA0"]
["1FK2103-4AG10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1239,"ΤΕΜ",1,"MC",1,"1FK21034AG100SA0"]
["1FK2103-4AG10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1560,"ΤΕΜ",1,"MC",1,"1FK21034AG101MA0"]
["1FK2103-4AG10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1239,"ΤΕΜ",1,"MC",1,"1FK21034AG101SA0"]
["1FK2103-4AG10-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1560,"ΤΕΜ",1,"MC",1,"1FK21034AG102MA0"]
["1FK2103-4AG10-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1239,"ΤΕΜ",1,"MC",1,"1FK21034AG102SA0"]
["1FK2103-4AG11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1650,"ΤΕΜ",1,"MC",1,"1FK21034AG110MA0"]
["1FK2103-4AG11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1329,"ΤΕΜ",1,"MC",1,"1FK21034AG110SA0"]
["1FK2103-4AG11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1650,"ΤΕΜ",1,"MC",1,"1FK21034AG111MA0"]
["1FK2103-4AG11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1329,"ΤΕΜ",1,"MC",1,"1FK21034AG111SA0"]
["1FK2103-4AG11-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M12, rotatable; .",1650,"ΤΕΜ",1,"MC",1,"1FK21034AG112MA0"]
["1FK2103-4AG11-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M12, rotatable; .",1329,"ΤΕΜ",1,"MC",1,"1FK21034AG112SA0"]
["1FK2104-4AF00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1303,"ΤΕΜ",1,"MC",1,"1FK21044AF000MA0"]
["1FK2104-4AF00-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1303,"ΤΕΜ",1,"MC",1,"1FK21044AF000MB0"]
["1FK2104-4AF00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",982,"ΤΕΜ",1,"MC",1,"1FK21044AF000SA0"]
["1FK2104-4AF00-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",982,"ΤΕΜ",1,"MC",1,"1FK21044AF000SB0"]
["1FK2104-4AF00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1303,"ΤΕΜ",1,"MC",1,"1FK21044AF001MA0"]
["1FK2104-4AF00-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1303,"ΤΕΜ",1,"MC",1,"1FK21044AF001MB0"]
["1FK2104-4AF00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",982,"ΤΕΜ",1,"MC",1,"1FK21044AF001SA0"]
["1FK2104-4AF00-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",982,"ΤΕΜ",1,"MC",1,"1FK21044AF001SB0"]
["1FK2104-4AF00-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1303,"ΤΕΜ",1,"MC",1,"1FK21044AF002MA0"]
["1FK2104-4AF00-2MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1303,"ΤΕΜ",1,"MC",1,"1FK21044AF002MB0"]
["1FK2104-4AF00-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",982,"ΤΕΜ",1,"MC",1,"1FK21044AF002SA0"]
["1FK2104-4AF00-2SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",982,"ΤΕΜ",1,"MC",1,"1FK21044AF002SB0"]
["1FK2104-4AF01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1393,"ΤΕΜ",1,"MC",1,"1FK21044AF010MA0"]
["1FK2104-4AF01-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1393,"ΤΕΜ",1,"MC",1,"1FK21044AF010MB0"]
["1FK2104-4AF01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1072,"ΤΕΜ",1,"MC",1,"1FK21044AF010SA0"]
["1FK2104-4AF01-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1072,"ΤΕΜ",1,"MC",1,"1FK21044AF010SB0"]
["1FK2104-4AF01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1393,"ΤΕΜ",1,"MC",1,"1FK21044AF011MA0"]
["1FK2104-4AF01-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1393,"ΤΕΜ",1,"MC",1,"1FK21044AF011MB0"]
["1FK2104-4AF01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1072,"ΤΕΜ",1,"MC",1,"1FK21044AF011SA0"]
["1FK2104-4AF01-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1072,"ΤΕΜ",1,"MC",1,"1FK21044AF011SB0"]
["1FK2104-4AF01-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480V); PN = 0.2 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1393,"ΤΕΜ",1,"MC",1,"1FK21044AF012MA0"]
["1FK2104-4AF01-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480V); PN = 0.2 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1393,"ΤΕΜ",1,"MC",1,"1FK21044AF012MB0"]
["1FK2104-4AF01-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480V); PN = 0.2 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1072,"ΤΕΜ",1,"MC",1,"1FK21044AF012SA0"]
["1FK2104-4AF01-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480V); PN = 0.2 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1072,"ΤΕΜ",1,"MC",1,"1FK21044AF012SB0"]
["1FK2104-4AF10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1560,"ΤΕΜ",1,"MC",1,"1FK21044AF100MA0"]
["1FK2104-4AF10-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1560,"ΤΕΜ",1,"MC",1,"1FK21044AF100MB0"]
["1FK2104-4AF10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1239,"ΤΕΜ",1,"MC",1,"1FK21044AF100SA0"]
["1FK2104-4AF10-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1239,"ΤΕΜ",1,"MC",1,"1FK21044AF100SB0"]
["1FK2104-4AF10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1560,"ΤΕΜ",1,"MC",1,"1FK21044AF101MA0"]
["1FK2104-4AF10-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1560,"ΤΕΜ",1,"MC",1,"1FK21044AF101MB0"]
["1FK2104-4AF10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1239,"ΤΕΜ",1,"MC",1,"1FK21044AF101SA0"]
["1FK2104-4AF10-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1239,"ΤΕΜ",1,"MC",1,"1FK21044AF101SB0"]
["1FK2104-4AF10-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1560,"ΤΕΜ",1,"MC",1,"1FK21044AF102MA0"]
["1FK2104-4AF10-2MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1560,"ΤΕΜ",1,"MC",1,"1FK21044AF102MB0"]
["1FK2104-4AF10-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1239,"ΤΕΜ",1,"MC",1,"1FK21044AF102SA0"]
["1FK2104-4AF10-2SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1239,"ΤΕΜ",1,"MC",1,"1FK21044AF102SB0"]
["1FK2104-4AF11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1650,"ΤΕΜ",1,"MC",1,"1FK21044AF110MA0"]
["1FK2104-4AF11-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1650,"ΤΕΜ",1,"MC",1,"1FK21044AF110MB0"]
["1FK2104-4AF11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1329,"ΤΕΜ",1,"MC",1,"1FK21044AF110SA0"]
["1FK2104-4AF11-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1329,"ΤΕΜ",1,"MC",1,"1FK21044AF110SB0"]
["1FK2104-4AF11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1650,"ΤΕΜ",1,"MC",1,"1FK21044AF111MA0"]
["1FK2104-4AF11-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1650,"ΤΕΜ",1,"MC",1,"1FK21044AF111MB0"]
["1FK2104-4AF11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1329,"ΤΕΜ",1,"MC",1,"1FK21044AF111SA0"]
["1FK2104-4AF11-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480 V); PN = 0.2 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1329,"ΤΕΜ",1,"MC",1,"1FK21044AF111SB0"]
["1FK2104-4AF11-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480V); PN = 0.2 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1650,"ΤΕΜ",1,"MC",1,"1FK21044AF112MA0"]
["1FK2104-4AF11-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480V); PN = 0.2 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1650,"ΤΕΜ",1,"MC",1,"1FK21044AF112MB0"]
["1FK2104-4AF11-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480V); PN = 0.2 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1329,"ΤΕΜ",1,"MC",1,"1FK21044AF112SA0"]
["1FK2104-4AF11-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (380-480V); PN = 0.2 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1329,"ΤΕΜ",1,"MC",1,"1FK21044AF112SB0"]
["1FK2104-4AK00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1303,"ΤΕΜ",1,"MC",1,"1FK21044AK000MA0"]
["1FK2104-4AK00-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1303,"ΤΕΜ",1,"MC",1,"1FK21044AK000MB0"]
["1FK2104-4AK00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",982,"ΤΕΜ",1,"MC",1,"1FK21044AK000SA0"]
["1FK2104-4AK00-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",982,"ΤΕΜ",1,"MC",1,"1FK21044AK000SB0"]
["1FK2104-4AK00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1303,"ΤΕΜ",1,"MC",1,"1FK21044AK001MA0"]
["1FK2104-4AK00-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1303,"ΤΕΜ",1,"MC",1,"1FK21044AK001MB0"]
["1FK2104-4AK00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",982,"ΤΕΜ",1,"MC",1,"1FK21044AK001SA0"]
["1FK2104-4AK00-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",982,"ΤΕΜ",1,"MC",1,"1FK21044AK001SB0"]
["1FK2104-4AK00-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1303,"ΤΕΜ",1,"MC",1,"1FK21044AK002MA0"]
["1FK2104-4AK00-2MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1303,"ΤΕΜ",1,"MC",1,"1FK21044AK002MB0"]
["1FK2104-4AK00-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",982,"ΤΕΜ",1,"MC",1,"1FK21044AK002SA0"]
["1FK2104-4AK00-2SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",982,"ΤΕΜ",1,"MC",1,"1FK21044AK002SB0"]
["1FK2104-4AK01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1393,"ΤΕΜ",1,"MC",1,"1FK21044AK010MA0"]
["1FK2104-4AK01-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1393,"ΤΕΜ",1,"MC",1,"1FK21044AK010MB0"]
["1FK2104-4AK01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1072,"ΤΕΜ",1,"MC",1,"1FK21044AK010SA0"]
["1FK2104-4AK01-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1072,"ΤΕΜ",1,"MC",1,"1FK21044AK010SB0"]
["1FK2104-4AK01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1393,"ΤΕΜ",1,"MC",1,"1FK21044AK011MA0"]
["1FK2104-4AK01-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1393,"ΤΕΜ",1,"MC",1,"1FK21044AK011MB0"]
["1FK2104-4AK01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1072,"ΤΕΜ",1,"MC",1,"1FK21044AK011SA0"]
["1FK2104-4AK01-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1072,"ΤΕΜ",1,"MC",1,"1FK21044AK011SB0"]
["1FK2104-4AK01-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480V); PN = 0.4 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1393,"ΤΕΜ",1,"MC",1,"1FK21044AK012MA0"]
["1FK2104-4AK01-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480V); PN = 0.4 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Βµs; .",1393,"ΤΕΜ",1,"MC",1,"1FK21044AK012MB0"]
["1FK2104-4AK01-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480V); PN = 0.4 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1072,"ΤΕΜ",1,"MC",1,"1FK21044AK012SA0"]
["1FK2104-4AK01-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480V); PN = 0.4 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Βµs; .",1072,"ΤΕΜ",1,"MC",1,"1FK21044AK012SB0"]
["1FK2104-4AK10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1560,"ΤΕΜ",1,"MC",1,"1FK21044AK100MA0"]
["1FK2104-4AK10-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1560,"ΤΕΜ",1,"MC",1,"1FK21044AK100MB0"]
["1FK2104-4AK10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1239,"ΤΕΜ",1,"MC",1,"1FK21044AK100SA0"]
["1FK2104-4AK10-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1239,"ΤΕΜ",1,"MC",1,"1FK21044AK100SB0"]
["1FK2104-4AK10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1560,"ΤΕΜ",1,"MC",1,"1FK21044AK101MA0"]
["1FK2104-4AK10-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1560,"ΤΕΜ",1,"MC",1,"1FK21044AK101MB0"]
["1FK2104-4AK10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1239,"ΤΕΜ",1,"MC",1,"1FK21044AK101SA0"]
["1FK2104-4AK10-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1239,"ΤΕΜ",1,"MC",1,"1FK21044AK101SB0"]
["1FK2104-4AK10-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1560,"ΤΕΜ",1,"MC",1,"1FK21044AK102MA0"]
["1FK2104-4AK10-2MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1560,"ΤΕΜ",1,"MC",1,"1FK21044AK102MB0"]
["1FK2104-4AK10-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1239,"ΤΕΜ",1,"MC",1,"1FK21044AK102SA0"]
["1FK2104-4AK10-2SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1239,"ΤΕΜ",1,"MC",1,"1FK21044AK102SB0"]
["1FK2104-4AK11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1650,"ΤΕΜ",1,"MC",1,"1FK21044AK110MA0"]
["1FK2104-4AK11-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1650,"ΤΕΜ",1,"MC",1,"1FK21044AK110MB0"]
["1FK2104-4AK11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1329,"ΤΕΜ",1,"MC",1,"1FK21044AK110SA0"]
["1FK2104-4AK11-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1329,"ΤΕΜ",1,"MC",1,"1FK21044AK110SB0"]
["1FK2104-4AK11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1650,"ΤΕΜ",1,"MC",1,"1FK21044AK111MA0"]
["1FK2104-4AK11-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1650,"ΤΕΜ",1,"MC",1,"1FK21044AK111MB0"]
["1FK2104-4AK11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1329,"ΤΕΜ",1,"MC",1,"1FK21044AK111SA0"]
["1FK2104-4AK11-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480 V); PN = 0.4 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1329,"ΤΕΜ",1,"MC",1,"1FK21044AK111SB0"]
["1FK2104-4AK11-2MA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480V); PN = 0.4 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1650,"ΤΕΜ",1,"MC",1,"1FK21044AK112MA0"]
["1FK2104-4AK11-2MB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480V); PN = 0.4 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Βµs; .",1650,"ΤΕΜ",1,"MC",1,"1FK21044AK112MB0"]
["1FK2104-4AK11-2SA0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480V); PN = 0.4 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1329,"ΤΕΜ",1,"MC",1,"1FK21044AK112SA0"]
["1FK2104-4AK11-2SB0","SIMOTICS S-1FK2 HD servo motor M0=1.27 Nm; PN = 0.6 kW at nN=6000 rpm (380-480V); PN = 0.4 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Βµs; .",1329,"ΤΕΜ",1,"MC",1,"1FK21044AK112SB0"]
["1FK2104-5AF00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1410,"ΤΕΜ",1,"MC",1,"1FK21045AF000MA0"]
["1FK2104-5AF00-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1410,"ΤΕΜ",1,"MC",1,"1FK21045AF000MB0"]
["1FK2104-5AF00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1089,"ΤΕΜ",1,"MC",1,"1FK21045AF000SA0"]
["1FK2104-5AF00-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1089,"ΤΕΜ",1,"MC",1,"1FK21045AF000SB0"]
["1FK2104-5AF00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1410,"ΤΕΜ",1,"MC",1,"1FK21045AF001MA0"]
["1FK2104-5AF00-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1410,"ΤΕΜ",1,"MC",1,"1FK21045AF001MB0"]
["1FK2104-5AF00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1089,"ΤΕΜ",1,"MC",1,"1FK21045AF001SA0"]
["1FK2104-5AF00-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1089,"ΤΕΜ",1,"MC",1,"1FK21045AF001SB0"]
["1FK2104-5AF00-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1410,"ΤΕΜ",1,"MC",1,"1FK21045AF002MA0"]
["1FK2104-5AF00-2MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1410,"ΤΕΜ",1,"MC",1,"1FK21045AF002MB0"]
["1FK2104-5AF00-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1089,"ΤΕΜ",1,"MC",1,"1FK21045AF002SA0"]
["1FK2104-5AF00-2SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1089,"ΤΕΜ",1,"MC",1,"1FK21045AF002SB0"]
["1FK2104-5AF01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1499,"ΤΕΜ",1,"MC",1,"1FK21045AF010MA0"]
["1FK2104-5AF01-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1499,"ΤΕΜ",1,"MC",1,"1FK21045AF010MB0"]
["1FK2104-5AF01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1178,"ΤΕΜ",1,"MC",1,"1FK21045AF010SA0"]
["1FK2104-5AF01-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1178,"ΤΕΜ",1,"MC",1,"1FK21045AF010SB0"]
["1FK2104-5AF01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1499,"ΤΕΜ",1,"MC",1,"1FK21045AF011MA0"]
["1FK2104-5AF01-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1499,"ΤΕΜ",1,"MC",1,"1FK21045AF011MB0"]
["1FK2104-5AF01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1178,"ΤΕΜ",1,"MC",1,"1FK21045AF011SA0"]
["1FK2104-5AF01-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1178,"ΤΕΜ",1,"MC",1,"1FK21045AF011SB0"]
["1FK2104-5AF01-2MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1499,"ΤΕΜ",1,"MC",1,"1FK21045AF012MA0"]
["1FK2104-5AF01-2MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1499,"ΤΕΜ",1,"MC",1,"1FK21045AF012MB0"]
["1FK2104-5AF01-2SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1178,"ΤΕΜ",1,"MC",1,"1FK21045AF012SA0"]
["1FK2104-5AF01-2SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1178,"ΤΕΜ",1,"MC",1,"1FK21045AF012SB0"]
["1FK2104-5AF10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1667,"ΤΕΜ",1,"MC",1,"1FK21045AF100MA0"]
["1FK2104-5AF10-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1667,"ΤΕΜ",1,"MC",1,"1FK21045AF100MB0"]
["1FK2104-5AF10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1346,"ΤΕΜ",1,"MC",1,"1FK21045AF100SA0"]
["1FK2104-5AF10-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1346,"ΤΕΜ",1,"MC",1,"1FK21045AF100SB0"]
["1FK2104-5AF10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1667,"ΤΕΜ",1,"MC",1,"1FK21045AF101MA0"]
["1FK2104-5AF10-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1667,"ΤΕΜ",1,"MC",1,"1FK21045AF101MB0"]
["1FK2104-5AF10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1346,"ΤΕΜ",1,"MC",1,"1FK21045AF101SA0"]
["1FK2104-5AF10-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1346,"ΤΕΜ",1,"MC",1,"1FK21045AF101SB0"]
["1FK2104-5AF10-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1667,"ΤΕΜ",1,"MC",1,"1FK21045AF102MA0"]
["1FK2104-5AF10-2MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1667,"ΤΕΜ",1,"MC",1,"1FK21045AF102MB0"]
["1FK2104-5AF10-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1346,"ΤΕΜ",1,"MC",1,"1FK21045AF102SA0"]
["1FK2104-5AF10-2SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1346,"ΤΕΜ",1,"MC",1,"1FK21045AF102SB0"]
["1FK2104-5AF11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1757,"ΤΕΜ",1,"MC",1,"1FK21045AF110MA0"]
["1FK2104-5AF11-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1757,"ΤΕΜ",1,"MC",1,"1FK21045AF110MB0"]
["1FK2104-5AF11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1436,"ΤΕΜ",1,"MC",1,"1FK21045AF110SA0"]
["1FK2104-5AF11-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1436,"ΤΕΜ",1,"MC",1,"1FK21045AF110SB0"]
["1FK2104-5AF11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1757,"ΤΕΜ",1,"MC",1,"1FK21045AF111MA0"]
["1FK2104-5AF11-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1757,"ΤΕΜ",1,"MC",1,"1FK21045AF111MB0"]
["1FK2104-5AF11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1436,"ΤΕΜ",1,"MC",1,"1FK21045AF111SA0"]
["1FK2104-5AF11-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1436,"ΤΕΜ",1,"MC",1,"1FK21045AF111SB0"]
["1FK2104-5AF11-2MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1757,"ΤΕΜ",1,"MC",1,"1FK21045AF112MA0"]
["1FK2104-5AF11-2MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1757,"ΤΕΜ",1,"MC",1,"1FK21045AF112MB0"]
["1FK2104-5AF11-2SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1436,"ΤΕΜ",1,"MC",1,"1FK21045AF112SA0"]
["1FK2104-5AF11-2SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1436,"ΤΕΜ",1,"MC",1,"1FK21045AF112SB0"]
["1FK2104-5AK00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1410,"ΤΕΜ",1,"MC",1,"1FK21045AK000MA0"]
["1FK2104-5AK00-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1410,"ΤΕΜ",1,"MC",1,"1FK21045AK000MB0"]
["1FK2104-5AK00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1089,"ΤΕΜ",1,"MC",1,"1FK21045AK000SA0"]
["1FK2104-5AK00-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1089,"ΤΕΜ",1,"MC",1,"1FK21045AK000SB0"]
["1FK2104-5AK00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1410,"ΤΕΜ",1,"MC",1,"1FK21045AK001MA0"]
["1FK2104-5AK00-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1410,"ΤΕΜ",1,"MC",1,"1FK21045AK001MB0"]
["1FK2104-5AK00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1089,"ΤΕΜ",1,"MC",1,"1FK21045AK001SA0"]
["1FK2104-5AK00-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1089,"ΤΕΜ",1,"MC",1,"1FK21045AK001SB0"]
["1FK2104-5AK00-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1410,"ΤΕΜ",1,"MC",1,"1FK21045AK002MA0"]
["1FK2104-5AK00-2MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1410,"ΤΕΜ",1,"MC",1,"1FK21045AK002MB0"]
["1FK2104-5AK00-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1089,"ΤΕΜ",1,"MC",1,"1FK21045AK002SA0"]
["1FK2104-5AK00-2SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1089,"ΤΕΜ",1,"MC",1,"1FK21045AK002SB0"]
["1FK2104-5AK01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1499,"ΤΕΜ",1,"MC",1,"1FK21045AK010MA0"]
["1FK2104-5AK01-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1499,"ΤΕΜ",1,"MC",1,"1FK21045AK010MB0"]
["1FK2104-5AK01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1178,"ΤΕΜ",1,"MC",1,"1FK21045AK010SA0"]
["1FK2104-5AK01-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1178,"ΤΕΜ",1,"MC",1,"1FK21045AK010SB0"]
["1FK2104-5AK01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1499,"ΤΕΜ",1,"MC",1,"1FK21045AK011MA0"]
["1FK2104-5AK01-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1499,"ΤΕΜ",1,"MC",1,"1FK21045AK011MB0"]
["1FK2104-5AK01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1178,"ΤΕΜ",1,"MC",1,"1FK21045AK011SA0"]
["1FK2104-5AK01-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1178,"ΤΕΜ",1,"MC",1,"1FK21045AK011SB0"]
["1FK2104-5AK01-2MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1499,"ΤΕΜ",1,"MC",1,"1FK21045AK012MA0"]
["1FK2104-5AK01-2MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Βµs; .",1499,"ΤΕΜ",1,"MC",1,"1FK21045AK012MB0"]
["1FK2104-5AK01-2SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1178,"ΤΕΜ",1,"MC",1,"1FK21045AK012SA0"]
["1FK2104-5AK01-2SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Βµs; .",1178,"ΤΕΜ",1,"MC",1,"1FK21045AK012SB0"]
["1FK2104-5AK10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1667,"ΤΕΜ",1,"MC",1,"1FK21045AK100MA0"]
["1FK2104-5AK10-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1667,"ΤΕΜ",1,"MC",1,"1FK21045AK100MB0"]
["1FK2104-5AK10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1346,"ΤΕΜ",1,"MC",1,"1FK21045AK100SA0"]
["1FK2104-5AK10-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1346,"ΤΕΜ",1,"MC",1,"1FK21045AK100SB0"]
["1FK2104-5AK10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1667,"ΤΕΜ",1,"MC",1,"1FK21045AK101MA0"]
["1FK2104-5AK10-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1667,"ΤΕΜ",1,"MC",1,"1FK21045AK101MB0"]
["1FK2104-5AK10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1346,"ΤΕΜ",1,"MC",1,"1FK21045AK101SA0"]
["1FK2104-5AK10-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1346,"ΤΕΜ",1,"MC",1,"1FK21045AK101SB0"]
["1FK2104-5AK10-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1667,"ΤΕΜ",1,"MC",1,"1FK21045AK102MA0"]
["1FK2104-5AK10-2MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1667,"ΤΕΜ",1,"MC",1,"1FK21045AK102MB0"]
["1FK2104-5AK10-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1346,"ΤΕΜ",1,"MC",1,"1FK21045AK102SA0"]
["1FK2104-5AK10-2SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1346,"ΤΕΜ",1,"MC",1,"1FK21045AK102SB0"]
["1FK2104-5AK11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1757,"ΤΕΜ",1,"MC",1,"1FK21045AK110MA0"]
["1FK2104-5AK11-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1757,"ΤΕΜ",1,"MC",1,"1FK21045AK110MB0"]
["1FK2104-5AK11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1436,"ΤΕΜ",1,"MC",1,"1FK21045AK110SA0"]
["1FK2104-5AK11-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1436,"ΤΕΜ",1,"MC",1,"1FK21045AK110SB0"]
["1FK2104-5AK11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1757,"ΤΕΜ",1,"MC",1,"1FK21045AK111MA0"]
["1FK2104-5AK11-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1757,"ΤΕΜ",1,"MC",1,"1FK21045AK111MB0"]
["1FK2104-5AK11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1436,"ΤΕΜ",1,"MC",1,"1FK21045AK111SA0"]
["1FK2104-5AK11-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1436,"ΤΕΜ",1,"MC",1,"1FK21045AK111SB0"]
["1FK2104-5AK11-2MA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1757,"ΤΕΜ",1,"MC",1,"1FK21045AK112MA0"]
["1FK2104-5AK11-2MB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Βµs; .",1757,"ΤΕΜ",1,"MC",1,"1FK21045AK112MB0"]
["1FK2104-5AK11-2SA0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1436,"ΤΕΜ",1,"MC",1,"1FK21045AK112SA0"]
["1FK2104-5AK11-2SB0","SIMOTICS S-1FK2 HD servo motor M0=2.4 Nm; PN = 1.07 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Βµs; .",1436,"ΤΕΜ",1,"MC",1,"1FK21045AK112SB0"]
["1FK2104-6AF00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1474,"ΤΕΜ",1,"MC",1,"1FK21046AF000MA0"]
["1FK2104-6AF00-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1474,"ΤΕΜ",1,"MC",1,"1FK21046AF000MB0"]
["1FK2104-6AF00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1153,"ΤΕΜ",1,"MC",1,"1FK21046AF000SA0"]
["1FK2104-6AF00-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1153,"ΤΕΜ",1,"MC",1,"1FK21046AF000SB0"]
["1FK2104-6AF00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1474,"ΤΕΜ",1,"MC",1,"1FK21046AF001MA0"]
["1FK2104-6AF00-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1474,"ΤΕΜ",1,"MC",1,"1FK21046AF001MB0"]
["1FK2104-6AF00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1153,"ΤΕΜ",1,"MC",1,"1FK21046AF001SA0"]
["1FK2104-6AF00-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1153,"ΤΕΜ",1,"MC",1,"1FK21046AF001SB0"]
["1FK2104-6AF00-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1474,"ΤΕΜ",1,"MC",1,"1FK21046AF002MA0"]
["1FK2104-6AF00-2MB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1474,"ΤΕΜ",1,"MC",1,"1FK21046AF002MB0"]
["1FK2104-6AF00-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1153,"ΤΕΜ",1,"MC",1,"1FK21046AF002SA0"]
["1FK2104-6AF00-2SB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1153,"ΤΕΜ",1,"MC",1,"1FK21046AF002SB0"]
["1FK2104-6AF01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1563,"ΤΕΜ",1,"MC",1,"1FK21046AF010MA0"]
["1FK2104-6AF01-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1563,"ΤΕΜ",1,"MC",1,"1FK21046AF010MB0"]
["1FK2104-6AF01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1242,"ΤΕΜ",1,"MC",1,"1FK21046AF010SA0"]
["1FK2104-6AF01-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1242,"ΤΕΜ",1,"MC",1,"1FK21046AF010SB0"]
["1FK2104-6AF01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1563,"ΤΕΜ",1,"MC",1,"1FK21046AF011MA0"]
["1FK2104-6AF01-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1563,"ΤΕΜ",1,"MC",1,"1FK21046AF011MB0"]
["1FK2104-6AF01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1242,"ΤΕΜ",1,"MC",1,"1FK21046AF011SA0"]
["1FK2104-6AF01-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1242,"ΤΕΜ",1,"MC",1,"1FK21046AF011SB0"]
["1FK2104-6AF01-2MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1563,"ΤΕΜ",1,"MC",1,"1FK21046AF012MA0"]
["1FK2104-6AF01-2MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1563,"ΤΕΜ",1,"MC",1,"1FK21046AF012MB0"]
["1FK2104-6AF01-2SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1242,"ΤΕΜ",1,"MC",1,"1FK21046AF012SA0"]
["1FK2104-6AF01-2SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1242,"ΤΕΜ",1,"MC",1,"1FK21046AF012SB0"]
["1FK2104-6AF10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1731,"ΤΕΜ",1,"MC",1,"1FK21046AF100MA0"]
["1FK2104-6AF10-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1731,"ΤΕΜ",1,"MC",1,"1FK21046AF100MB0"]
["1FK2104-6AF10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1410,"ΤΕΜ",1,"MC",1,"1FK21046AF100SA0"]
["1FK2104-6AF10-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1410,"ΤΕΜ",1,"MC",1,"1FK21046AF100SB0"]
["1FK2104-6AF10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1731,"ΤΕΜ",1,"MC",1,"1FK21046AF101MA0"]
["1FK2104-6AF10-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1731,"ΤΕΜ",1,"MC",1,"1FK21046AF101MB0"]
["1FK2104-6AF10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1410,"ΤΕΜ",1,"MC",1,"1FK21046AF101SA0"]
["1FK2104-6AF10-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1410,"ΤΕΜ",1,"MC",1,"1FK21046AF101SB0"]
["1FK2104-6AF10-2MA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1731,"ΤΕΜ",1,"MC",1,"1FK21046AF102MA0"]
["1FK2104-6AF10-2MB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1731,"ΤΕΜ",1,"MC",1,"1FK21046AF102MB0"]
["1FK2104-6AF10-2SA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1410,"ΤΕΜ",1,"MC",1,"1FK21046AF102SA0"]
["1FK2104-6AF10-2SB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1410,"ΤΕΜ",1,"MC",1,"1FK21046AF102SB0"]
["1FK2104-6AF11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1821,"ΤΕΜ",1,"MC",1,"1FK21046AF110MA0"]
["1FK2104-6AF11-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1821,"ΤΕΜ",1,"MC",1,"1FK21046AF110MB0"]
["1FK2104-6AF11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1500,"ΤΕΜ",1,"MC",1,"1FK21046AF110SA0"]
["1FK2104-6AF11-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1500,"ΤΕΜ",1,"MC",1,"1FK21046AF110SB0"]
["1FK2104-6AF11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1821,"ΤΕΜ",1,"MC",1,"1FK21046AF111MA0"]
["1FK2104-6AF11-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1821,"ΤΕΜ",1,"MC",1,"1FK21046AF111MB0"]
["1FK2104-6AF11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1500,"ΤΕΜ",1,"MC",1,"1FK21046AF111SA0"]
["1FK2104-6AF11-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1500,"ΤΕΜ",1,"MC",1,"1FK21046AF111SB0"]
["1FK2104-6AF11-2MA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1821,"ΤΕΜ",1,"MC",1,"1FK21046AF112MA0"]
["1FK2104-6AF11-2MB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1821,"ΤΕΜ",1,"MC",1,"1FK21046AF112MB0"]
["1FK2104-6AF11-2SA0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1500,"ΤΕΜ",1,"MC",1,"1FK21046AF112SA0"]
["1FK2104-6AF11-2SB0","SIMOTICS S-1FK2 HD servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1500,"ΤΕΜ",1,"MC",1,"1FK21046AF112SB0"]
["1FK2105-4AF00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1640,"ΤΕΜ",1,"MC",1,"1FK21054AF000MA0"]
["1FK2105-4AF00-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1640,"ΤΕΜ",1,"MC",1,"1FK21054AF000MB0"]
["1FK2105-4AF00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1319,"ΤΕΜ",1,"MC",1,"1FK21054AF000SA0"]
["1FK2105-4AF00-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1319,"ΤΕΜ",1,"MC",1,"1FK21054AF000SB0"]
["1FK2105-4AF00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1640,"ΤΕΜ",1,"MC",1,"1FK21054AF001MA0"]
["1FK2105-4AF00-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1640,"ΤΕΜ",1,"MC",1,"1FK21054AF001MB0"]
["1FK2105-4AF00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1319,"ΤΕΜ",1,"MC",1,"1FK21054AF001SA0"]
["1FK2105-4AF00-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1319,"ΤΕΜ",1,"MC",1,"1FK21054AF001SB0"]
["1FK2105-4AF01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1730,"ΤΕΜ",1,"MC",1,"1FK21054AF010MA0"]
["1FK2105-4AF01-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1730,"ΤΕΜ",1,"MC",1,"1FK21054AF010MB0"]
["1FK2105-4AF01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1409,"ΤΕΜ",1,"MC",1,"1FK21054AF010SA0"]
["1FK2105-4AF01-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1409,"ΤΕΜ",1,"MC",1,"1FK21054AF010SB0"]
["1FK2105-4AF01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1730,"ΤΕΜ",1,"MC",1,"1FK21054AF011MA0"]
["1FK2105-4AF01-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1730,"ΤΕΜ",1,"MC",1,"1FK21054AF011MB0"]
["1FK2105-4AF01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1409,"ΤΕΜ",1,"MC",1,"1FK21054AF011SA0"]
["1FK2105-4AF01-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1409,"ΤΕΜ",1,"MC",1,"1FK21054AF011SB0"]
["1FK2105-4AF10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1941,"ΤΕΜ",1,"MC",1,"1FK21054AF100MA0"]
["1FK2105-4AF10-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1941,"ΤΕΜ",1,"MC",1,"1FK21054AF100MB0"]
["1FK2105-4AF10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1620,"ΤΕΜ",1,"MC",1,"1FK21054AF100SA0"]
["1FK2105-4AF10-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1620,"ΤΕΜ",1,"MC",1,"1FK21054AF100SB0"]
["1FK2105-4AF10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1941,"ΤΕΜ",1,"MC",1,"1FK21054AF101MA0"]
["1FK2105-4AF10-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1941,"ΤΕΜ",1,"MC",1,"1FK21054AF101MB0"]
["1FK2105-4AF10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1620,"ΤΕΜ",1,"MC",1,"1FK21054AF101SA0"]
["1FK2105-4AF10-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1620,"ΤΕΜ",1,"MC",1,"1FK21054AF101SB0"]
["1FK2105-4AF11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",2030,"ΤΕΜ",1,"MC",1,"1FK21054AF110MA0"]
["1FK2105-4AF11-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",2030,"ΤΕΜ",1,"MC",1,"1FK21054AF110MB0"]
["1FK2105-4AF11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1709,"ΤΕΜ",1,"MC",1,"1FK21054AF110SA0"]
["1FK2105-4AF11-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1709,"ΤΕΜ",1,"MC",1,"1FK21054AF110SB0"]
["1FK2105-4AF11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",2030,"ΤΕΜ",1,"MC",1,"1FK21054AF111MA0"]
["1FK2105-4AF11-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",2030,"ΤΕΜ",1,"MC",1,"1FK21054AF111MB0"]
["1FK2105-4AF11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1709,"ΤΕΜ",1,"MC",1,"1FK21054AF111SA0"]
["1FK2105-4AF11-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=5 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.79 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1709,"ΤΕΜ",1,"MC",1,"1FK21054AF111SB0"]
["1FK2105-6AF00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1900,"ΤΕΜ",1,"MC",1,"1FK21056AF000MA0"]
["1FK2105-6AF00-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1900,"ΤΕΜ",1,"MC",1,"1FK21056AF000MB0"]
["1FK2105-6AF00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1579,"ΤΕΜ",1,"MC",1,"1FK21056AF000SA0"]
["1FK2105-6AF00-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1579,"ΤΕΜ",1,"MC",1,"1FK21056AF000SB0"]
["1FK2105-6AF00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1900,"ΤΕΜ",1,"MC",1,"1FK21056AF001MA0"]
["1FK2105-6AF00-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1900,"ΤΕΜ",1,"MC",1,"1FK21056AF001MB0"]
["1FK2105-6AF00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1579,"ΤΕΜ",1,"MC",1,"1FK21056AF001SA0"]
["1FK2105-6AF00-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1579,"ΤΕΜ",1,"MC",1,"1FK21056AF001SB0"]
["1FK2105-6AF01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1990,"ΤΕΜ",1,"MC",1,"1FK21056AF010MA0"]
["1FK2105-6AF01-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1990,"ΤΕΜ",1,"MC",1,"1FK21056AF010MB0"]
["1FK2105-6AF01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1669,"ΤΕΜ",1,"MC",1,"1FK21056AF010SA0"]
["1FK2105-6AF01-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1669,"ΤΕΜ",1,"MC",1,"1FK21056AF010SB0"]
["1FK2105-6AF01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1990,"ΤΕΜ",1,"MC",1,"1FK21056AF011MA0"]
["1FK2105-6AF01-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1990,"ΤΕΜ",1,"MC",1,"1FK21056AF011MB0"]
["1FK2105-6AF01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1669,"ΤΕΜ",1,"MC",1,"1FK21056AF011SA0"]
["1FK2105-6AF01-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1669,"ΤΕΜ",1,"MC",1,"1FK21056AF011SB0"]
["1FK2105-6AF10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",2201,"ΤΕΜ",1,"MC",1,"1FK21056AF100MA0"]
["1FK2105-6AF10-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",2201,"ΤΕΜ",1,"MC",1,"1FK21056AF100MB0"]
["1FK2105-6AF10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1880,"ΤΕΜ",1,"MC",1,"1FK21056AF100SA0"]
["1FK2105-6AF10-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1880,"ΤΕΜ",1,"MC",1,"1FK21056AF100SB0"]
["1FK2105-6AF10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",2201,"ΤΕΜ",1,"MC",1,"1FK21056AF101MA0"]
["1FK2105-6AF10-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",2201,"ΤΕΜ",1,"MC",1,"1FK21056AF101MB0"]
["1FK2105-6AF10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1880,"ΤΕΜ",1,"MC",1,"1FK21056AF101SA0"]
["1FK2105-6AF10-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1880,"ΤΕΜ",1,"MC",1,"1FK21056AF101SB0"]
["1FK2105-6AF11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",2290,"ΤΕΜ",1,"MC",1,"1FK21056AF110MA0"]
["1FK2105-6AF11-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",2290,"ΤΕΜ",1,"MC",1,"1FK21056AF110MB0"]
["1FK2105-6AF11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1969,"ΤΕΜ",1,"MC",1,"1FK21056AF110SA0"]
["1FK2105-6AF11-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1969,"ΤΕΜ",1,"MC",1,"1FK21056AF110SB0"]
["1FK2105-6AF11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",2290,"ΤΕΜ",1,"MC",1,"1FK21056AF111MA0"]
["1FK2105-6AF11-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",2290,"ΤΕΜ",1,"MC",1,"1FK21056AF111MB0"]
["1FK2105-6AF11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1969,"ΤΕΜ",1,"MC",1,"1FK21056AF111SA0"]
["1FK2105-6AF11-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=8 Nm; PN = 2.1 kW at nN=3000 rpm (380-480 V); PN = 1.26 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1969,"ΤΕΜ",1,"MC",1,"1FK21056AF111SB0"]
["1FK2106-3AF00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",1960,"ΤΕΜ",1,"MC",1,"1FK21063AF000MA0"]
["1FK2106-3AF00-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1960,"ΤΕΜ",1,"MC",1,"1FK21063AF000MB0"]
["1FK2106-3AF00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1639,"ΤΕΜ",1,"MC",1,"1FK21063AF000SA0"]
["1FK2106-3AF00-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1639,"ΤΕΜ",1,"MC",1,"1FK21063AF000SB0"]
["1FK2106-3AF00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",1960,"ΤΕΜ",1,"MC",1,"1FK21063AF001MA0"]
["1FK2106-3AF00-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1960,"ΤΕΜ",1,"MC",1,"1FK21063AF001MB0"]
["1FK2106-3AF00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1639,"ΤΕΜ",1,"MC",1,"1FK21063AF001SA0"]
["1FK2106-3AF00-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1639,"ΤΕΜ",1,"MC",1,"1FK21063AF001SB0"]
["1FK2106-3AF01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2050,"ΤΕΜ",1,"MC",1,"1FK21063AF010MA0"]
["1FK2106-3AF01-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2050,"ΤΕΜ",1,"MC",1,"1FK21063AF010MB0"]
["1FK2106-3AF01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1729,"ΤΕΜ",1,"MC",1,"1FK21063AF010SA0"]
["1FK2106-3AF01-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1729,"ΤΕΜ",1,"MC",1,"1FK21063AF010SB0"]
["1FK2106-3AF01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2050,"ΤΕΜ",1,"MC",1,"1FK21063AF011MA0"]
["1FK2106-3AF01-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2050,"ΤΕΜ",1,"MC",1,"1FK21063AF011MB0"]
["1FK2106-3AF01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1729,"ΤΕΜ",1,"MC",1,"1FK21063AF011SA0"]
["1FK2106-3AF01-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1729,"ΤΕΜ",1,"MC",1,"1FK21063AF011SB0"]
["1FK2106-3AF10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2303,"ΤΕΜ",1,"MC",1,"1FK21063AF100MA0"]
["1FK2106-3AF10-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2303,"ΤΕΜ",1,"MC",1,"1FK21063AF100MB0"]
["1FK2106-3AF10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1982,"ΤΕΜ",1,"MC",1,"1FK21063AF100SA0"]
["1FK2106-3AF10-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1982,"ΤΕΜ",1,"MC",1,"1FK21063AF100SB0"]
["1FK2106-3AF10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2303,"ΤΕΜ",1,"MC",1,"1FK21063AF101MA0"]
["1FK2106-3AF10-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2303,"ΤΕΜ",1,"MC",1,"1FK21063AF101MB0"]
["1FK2106-3AF10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1982,"ΤΕΜ",1,"MC",1,"1FK21063AF101SA0"]
["1FK2106-3AF10-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1982,"ΤΕΜ",1,"MC",1,"1FK21063AF101SB0"]
["1FK2106-3AF11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2393,"ΤΕΜ",1,"MC",1,"1FK21063AF110MA0"]
["1FK2106-3AF11-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2393,"ΤΕΜ",1,"MC",1,"1FK21063AF110MB0"]
["1FK2106-3AF11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2072,"ΤΕΜ",1,"MC",1,"1FK21063AF110SA0"]
["1FK2106-3AF11-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2072,"ΤΕΜ",1,"MC",1,"1FK21063AF110SB0"]
["1FK2106-3AF11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2393,"ΤΕΜ",1,"MC",1,"1FK21063AF111MA0"]
["1FK2106-3AF11-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2393,"ΤΕΜ",1,"MC",1,"1FK21063AF111MB0"]
["1FK2106-3AF11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2072,"ΤΕΜ",1,"MC",1,"1FK21063AF111SA0"]
["1FK2106-3AF11-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=9 Nm; PN = 2.3 kW at nN=3000 rpm (380-480 V); PN = 1.3 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2072,"ΤΕΜ",1,"MC",1,"1FK21063AF111SB0"]
["1FK2106-4AF00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2108,"ΤΕΜ",1,"MC",1,"1FK21064AF000MA0"]
["1FK2106-4AF00-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2108,"ΤΕΜ",1,"MC",1,"1FK21064AF000MB0"]
["1FK2106-4AF00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1787,"ΤΕΜ",1,"MC",1,"1FK21064AF000SA0"]
["1FK2106-4AF00-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1787,"ΤΕΜ",1,"MC",1,"1FK21064AF000SB0"]
["1FK2106-4AF00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2108,"ΤΕΜ",1,"MC",1,"1FK21064AF001MA0"]
["1FK2106-4AF00-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2108,"ΤΕΜ",1,"MC",1,"1FK21064AF001MB0"]
["1FK2106-4AF00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1787,"ΤΕΜ",1,"MC",1,"1FK21064AF001SA0"]
["1FK2106-4AF00-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1787,"ΤΕΜ",1,"MC",1,"1FK21064AF001SB0"]
["1FK2106-4AF01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2197,"ΤΕΜ",1,"MC",1,"1FK21064AF010MA0"]
["1FK2106-4AF01-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2197,"ΤΕΜ",1,"MC",1,"1FK21064AF010MB0"]
["1FK2106-4AF01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1876,"ΤΕΜ",1,"MC",1,"1FK21064AF010SA0"]
["1FK2106-4AF01-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1876,"ΤΕΜ",1,"MC",1,"1FK21064AF010SB0"]
["1FK2106-4AF01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2197,"ΤΕΜ",1,"MC",1,"1FK21064AF011MA0"]
["1FK2106-4AF01-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2197,"ΤΕΜ",1,"MC",1,"1FK21064AF011MB0"]
["1FK2106-4AF01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1876,"ΤΕΜ",1,"MC",1,"1FK21064AF011SA0"]
["1FK2106-4AF01-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1876,"ΤΕΜ",1,"MC",1,"1FK21064AF011SB0"]
["1FK2106-4AF10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2451,"ΤΕΜ",1,"MC",1,"1FK21064AF100MA0"]
["1FK2106-4AF10-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2451,"ΤΕΜ",1,"MC",1,"1FK21064AF100MB0"]
["1FK2106-4AF10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2130,"ΤΕΜ",1,"MC",1,"1FK21064AF100SA0"]
["1FK2106-4AF10-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2130,"ΤΕΜ",1,"MC",1,"1FK21064AF100SB0"]
["1FK2106-4AF10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2451,"ΤΕΜ",1,"MC",1,"1FK21064AF101MA0"]
["1FK2106-4AF10-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2451,"ΤΕΜ",1,"MC",1,"1FK21064AF101MB0"]
["1FK2106-4AF10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2130,"ΤΕΜ",1,"MC",1,"1FK21064AF101SA0"]
["1FK2106-4AF10-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2130,"ΤΕΜ",1,"MC",1,"1FK21064AF101SB0"]
["1FK2106-4AF11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2541,"ΤΕΜ",1,"MC",1,"1FK21064AF110MA0"]
["1FK2106-4AF11-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2541,"ΤΕΜ",1,"MC",1,"1FK21064AF110MB0"]
["1FK2106-4AF11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2220,"ΤΕΜ",1,"MC",1,"1FK21064AF110SA0"]
["1FK2106-4AF11-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2220,"ΤΕΜ",1,"MC",1,"1FK21064AF110SB0"]
["1FK2106-4AF11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2541,"ΤΕΜ",1,"MC",1,"1FK21064AF111MA0"]
["1FK2106-4AF11-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2541,"ΤΕΜ",1,"MC",1,"1FK21064AF111MB0"]
["1FK2106-4AF11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2220,"ΤΕΜ",1,"MC",1,"1FK21064AF111SA0"]
["1FK2106-4AF11-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=12 Nm; PN = 2.7 kW at nN=3000 rpm (380-480 V); PN = 1.64 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2220,"ΤΕΜ",1,"MC",1,"1FK21064AF111SB0"]
["1FK2106-6AF00-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2424,"ΤΕΜ",1,"MC",1,"1FK21066AF000MA0"]
["1FK2106-6AF00-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2424,"ΤΕΜ",1,"MC",1,"1FK21066AF000MB0"]
["1FK2106-6AF00-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2103,"ΤΕΜ",1,"MC",1,"1FK21066AF000SA0"]
["1FK2106-6AF00-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2103,"ΤΕΜ",1,"MC",1,"1FK21066AF000SB0"]
["1FK2106-6AF00-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2424,"ΤΕΜ",1,"MC",1,"1FK21066AF001MA0"]
["1FK2106-6AF00-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2424,"ΤΕΜ",1,"MC",1,"1FK21066AF001MB0"]
["1FK2106-6AF00-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2103,"ΤΕΜ",1,"MC",1,"1FK21066AF001SA0"]
["1FK2106-6AF00-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2103,"ΤΕΜ",1,"MC",1,"1FK21066AF001SB0"]
["1FK2106-6AF01-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2514,"ΤΕΜ",1,"MC",1,"1FK21066AF010MA0"]
["1FK2106-6AF01-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2514,"ΤΕΜ",1,"MC",1,"1FK21066AF010MB0"]
["1FK2106-6AF01-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2192,"ΤΕΜ",1,"MC",1,"1FK21066AF010SA0"]
["1FK2106-6AF01-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2192,"ΤΕΜ",1,"MC",1,"1FK21066AF010SB0"]
["1FK2106-6AF01-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2514,"ΤΕΜ",1,"MC",1,"1FK21066AF011MA0"]
["1FK2106-6AF01-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2514,"ΤΕΜ",1,"MC",1,"1FK21066AF011MB0"]
["1FK2106-6AF01-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2192,"ΤΕΜ",1,"MC",1,"1FK21066AF011SA0"]
["1FK2106-6AF01-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2192,"ΤΕΜ",1,"MC",1,"1FK21066AF011SB0"]
["1FK2106-6AF10-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2767,"ΤΕΜ",1,"MC",1,"1FK21066AF100MA0"]
["1FK2106-6AF10-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2767,"ΤΕΜ",1,"MC",1,"1FK21066AF100MB0"]
["1FK2106-6AF10-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2446,"ΤΕΜ",1,"MC",1,"1FK21066AF100SA0"]
["1FK2106-6AF10-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2446,"ΤΕΜ",1,"MC",1,"1FK21066AF100SB0"]
["1FK2106-6AF10-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2767,"ΤΕΜ",1,"MC",1,"1FK21066AF101MA0"]
["1FK2106-6AF10-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2767,"ΤΕΜ",1,"MC",1,"1FK21066AF101MB0"]
["1FK2106-6AF10-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2446,"ΤΕΜ",1,"MC",1,"1FK21066AF101SA0"]
["1FK2106-6AF10-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2446,"ΤΕΜ",1,"MC",1,"1FK21066AF101SB0"]
["1FK2106-6AF11-0MA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2857,"ΤΕΜ",1,"MC",1,"1FK21066AF110MA0"]
["1FK2106-6AF11-0MB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2857,"ΤΕΜ",1,"MC",1,"1FK21066AF110MB0"]
["1FK2106-6AF11-0SA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2536,"ΤΕΜ",1,"MC",1,"1FK21066AF110SA0"]
["1FK2106-6AF11-0SB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2536,"ΤΕΜ",1,"MC",1,"1FK21066AF110SB0"]
["1FK2106-6AF11-1MA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2857,"ΤΕΜ",1,"MC",1,"1FK21066AF111MA0"]
["1FK2106-6AF11-1MB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2857,"ΤΕΜ",1,"MC",1,"1FK21066AF111MB0"]
["1FK2106-6AF11-1SA0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2536,"ΤΕΜ",1,"MC",1,"1FK21066AF111SA0"]
["1FK2106-6AF11-1SB0","SIMOTICS S-1FK2 HD Servo motor M0=16 Nm; PN = 3.3 kW at nN=3000 rpm (380-480 V); PN = 2.15 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2536,"ΤΕΜ",1,"MC",1,"1FK21066AF111SB0"]
["1FK2203-2AG00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1175,"ΤΕΜ",1,"MC",1,"1FK22032AG000MA0"]
["1FK2203-2AG00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",854,"ΤΕΜ",1,"MC",1,"1FK22032AG000SA0"]
["1FK2203-2AG00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1175,"ΤΕΜ",1,"MC",1,"1FK22032AG001MA0"]
["1FK2203-2AG00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",854,"ΤΕΜ",1,"MC",1,"1FK22032AG001SA0"]
["1FK2203-2AG00-2MA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1175,"ΤΕΜ",1,"MC",1,"1FK22032AG002MA0"]
["1FK2203-2AG00-2SA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",854,"ΤΕΜ",1,"MC",1,"1FK22032AG002SA0"]
["1FK2203-2AG01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1265,"ΤΕΜ",1,"MC",1,"1FK22032AG010MA0"]
["1FK2203-2AG01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",944,"ΤΕΜ",1,"MC",1,"1FK22032AG010SA0"]
["1FK2203-2AG01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1265,"ΤΕΜ",1,"MC",1,"1FK22032AG011MA0"]
["1FK2203-2AG01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",944,"ΤΕΜ",1,"MC",1,"1FK22032AG011SA0"]
["1FK2203-2AG01-2MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M12, rotatable; .",1265,"ΤΕΜ",1,"MC",1,"1FK22032AG012MA0"]
["1FK2203-2AG01-2SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M12, rotatable; .",944,"ΤΕΜ",1,"MC",1,"1FK22032AG012SA0"]
["1FK2203-2AG10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1432,"ΤΕΜ",1,"MC",1,"1FK22032AG100MA0"]
["1FK2203-2AG10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1111,"ΤΕΜ",1,"MC",1,"1FK22032AG100SA0"]
["1FK2203-2AG10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1432,"ΤΕΜ",1,"MC",1,"1FK22032AG101MA0"]
["1FK2203-2AG10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1111,"ΤΕΜ",1,"MC",1,"1FK22032AG101SA0"]
["1FK2203-2AG10-2MA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1432,"ΤΕΜ",1,"MC",1,"1FK22032AG102MA0"]
["1FK2203-2AG10-2SA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1111,"ΤΕΜ",1,"MC",1,"1FK22032AG102SA0"]
["1FK2203-2AG11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1522,"ΤΕΜ",1,"MC",1,"1FK22032AG110MA0"]
["1FK2203-2AG11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1201,"ΤΕΜ",1,"MC",1,"1FK22032AG110SA0"]
["1FK2203-2AG11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1522,"ΤΕΜ",1,"MC",1,"1FK22032AG111MA0"]
["1FK2203-2AG11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1201,"ΤΕΜ",1,"MC",1,"1FK22032AG111SA0"]
["1FK2203-2AG11-2MA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M12, rotatable; .",1522,"ΤΕΜ",1,"MC",1,"1FK22032AG112MA0"]
["1FK2203-2AG11-2SA0","SIMOTICS S-1FK2 CT servo motor M0=0.64 Nm; PN = 0.2 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M12, rotatable; .",1201,"ΤΕΜ",1,"MC",1,"1FK22032AG112SA0"]
["1FK2203-4AG00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1303,"ΤΕΜ",1,"MC",1,"1FK22034AG000MA0"]
["1FK2203-4AG00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",982,"ΤΕΜ",1,"MC",1,"1FK22034AG000SA0"]
["1FK2203-4AG00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1303,"ΤΕΜ",1,"MC",1,"1FK22034AG001MA0"]
["1FK2203-4AG00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",982,"ΤΕΜ",1,"MC",1,"1FK22034AG001SA0"]
["1FK2203-4AG00-2MA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1303,"ΤΕΜ",1,"MC",1,"1FK22034AG002MA0"]
["1FK2203-4AG00-2SA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",982,"ΤΕΜ",1,"MC",1,"1FK22034AG002SA0"]
["1FK2203-4AG01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1393,"ΤΕΜ",1,"MC",1,"1FK22034AG010MA0"]
["1FK2203-4AG01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1072,"ΤΕΜ",1,"MC",1,"1FK22034AG010SA0"]
["1FK2203-4AG01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1393,"ΤΕΜ",1,"MC",1,"1FK22034AG011MA0"]
["1FK2203-4AG01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1072,"ΤΕΜ",1,"MC",1,"1FK22034AG011SA0"]
["1FK2203-4AG01-2MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M12, rotatable; .",1393,"ΤΕΜ",1,"MC",1,"1FK22034AG012MA0"]
["1FK2203-4AG01-2SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M12, rotatable; .",1072,"ΤΕΜ",1,"MC",1,"1FK22034AG012SA0"]
["1FK2203-4AG10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1560,"ΤΕΜ",1,"MC",1,"1FK22034AG100MA0"]
["1FK2203-4AG10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1239,"ΤΕΜ",1,"MC",1,"1FK22034AG100SA0"]
["1FK2203-4AG10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1560,"ΤΕΜ",1,"MC",1,"1FK22034AG101MA0"]
["1FK2203-4AG10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1239,"ΤΕΜ",1,"MC",1,"1FK22034AG101SA0"]
["1FK2203-4AG10-2MA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1560,"ΤΕΜ",1,"MC",1,"1FK22034AG102MA0"]
["1FK2203-4AG10-2SA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D11 x 23 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1239,"ΤΕΜ",1,"MC",1,"1FK22034AG102SA0"]
["1FK2203-4AG11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1650,"ΤΕΜ",1,"MC",1,"1FK22034AG110MA0"]
["1FK2203-4AG11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1329,"ΤΕΜ",1,"MC",1,"1FK22034AG110SA0"]
["1FK2203-4AG11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M12, rotatable;",1650,"ΤΕΜ",1,"MC",1,"1FK22034AG111MA0"]
["1FK2203-4AG11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D14x30 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M12, rotatable;",1329,"ΤΕΜ",1,"MC",1,"1FK22034AG111SA0"]
["1FK2203-4AG11-2MA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M12, rotatable; .",1650,"ΤΕΜ",1,"MC",1,"1FK22034AG112MA0"]
["1FK2203-4AG11-2SA0","SIMOTICS S-1FK2 CT servo motor M0=1.27 Nm; PN = 0.4 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D11 x 23 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M12, rotatable; .",1329,"ΤΕΜ",1,"MC",1,"1FK22034AG112SA0"]
["1FK2204-5AF00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1410,"ΤΕΜ",1,"MC",1,"1FK22045AF000MA0"]
["1FK2204-5AF00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1410,"ΤΕΜ",1,"MC",1,"1FK22045AF000MB0"]
["1FK2204-5AF00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1089,"ΤΕΜ",1,"MC",1,"1FK22045AF000SA0"]
["1FK2204-5AF00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1089,"ΤΕΜ",1,"MC",1,"1FK22045AF000SB0"]
["1FK2204-5AF00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1410,"ΤΕΜ",1,"MC",1,"1FK22045AF001MA0"]
["1FK2204-5AF00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1410,"ΤΕΜ",1,"MC",1,"1FK22045AF001MB0"]
["1FK2204-5AF00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1089,"ΤΕΜ",1,"MC",1,"1FK22045AF001SA0"]
["1FK2204-5AF00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1089,"ΤΕΜ",1,"MC",1,"1FK22045AF001SB0"]
["1FK2204-5AF00-2MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1410,"ΤΕΜ",1,"MC",1,"1FK22045AF002MA0"]
["1FK2204-5AF00-2MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1410,"ΤΕΜ",1,"MC",1,"1FK22045AF002MB0"]
["1FK2204-5AF00-2SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1089,"ΤΕΜ",1,"MC",1,"1FK22045AF002SA0"]
["1FK2204-5AF00-2SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1089,"ΤΕΜ",1,"MC",1,"1FK22045AF002SB0"]
["1FK2204-5AF01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1499,"ΤΕΜ",1,"MC",1,"1FK22045AF010MA0"]
["1FK2204-5AF01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1499,"ΤΕΜ",1,"MC",1,"1FK22045AF010MB0"]
["1FK2204-5AF01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1178,"ΤΕΜ",1,"MC",1,"1FK22045AF010SA0"]
["1FK2204-5AF01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1178,"ΤΕΜ",1,"MC",1,"1FK22045AF010SB0"]
["1FK2204-5AF01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1499,"ΤΕΜ",1,"MC",1,"1FK22045AF011MA0"]
["1FK2204-5AF01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1499,"ΤΕΜ",1,"MC",1,"1FK22045AF011MB0"]
["1FK2204-5AF01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1178,"ΤΕΜ",1,"MC",1,"1FK22045AF011SA0"]
["1FK2204-5AF01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1178,"ΤΕΜ",1,"MC",1,"1FK22045AF011SB0"]
["1FK2204-5AF01-2MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1499,"ΤΕΜ",1,"MC",1,"1FK22045AF012MA0"]
["1FK2204-5AF01-2MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1499,"ΤΕΜ",1,"MC",1,"1FK22045AF012MB0"]
["1FK2204-5AF01-2SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1178,"ΤΕΜ",1,"MC",1,"1FK22045AF012SA0"]
["1FK2204-5AF01-2SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1178,"ΤΕΜ",1,"MC",1,"1FK22045AF012SB0"]
["1FK2204-5AF10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1667,"ΤΕΜ",1,"MC",1,"1FK22045AF100MA0"]
["1FK2204-5AF10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1667,"ΤΕΜ",1,"MC",1,"1FK22045AF100MB0"]
["1FK2204-5AF10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1346,"ΤΕΜ",1,"MC",1,"1FK22045AF100SA0"]
["1FK2204-5AF10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1346,"ΤΕΜ",1,"MC",1,"1FK22045AF100SB0"]
["1FK2204-5AF10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1667,"ΤΕΜ",1,"MC",1,"1FK22045AF101MA0"]
["1FK2204-5AF10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1667,"ΤΕΜ",1,"MC",1,"1FK22045AF101MB0"]
["1FK2204-5AF10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1346,"ΤΕΜ",1,"MC",1,"1FK22045AF101SA0"]
["1FK2204-5AF10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1346,"ΤΕΜ",1,"MC",1,"1FK22045AF101SB0"]
["1FK2204-5AF10-2MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1667,"ΤΕΜ",1,"MC",1,"1FK22045AF102MA0"]
["1FK2204-5AF10-2MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1667,"ΤΕΜ",1,"MC",1,"1FK22045AF102MB0"]
["1FK2204-5AF10-2SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1346,"ΤΕΜ",1,"MC",1,"1FK22045AF102SA0"]
["1FK2204-5AF10-2SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1346,"ΤΕΜ",1,"MC",1,"1FK22045AF102SB0"]
["1FK2204-5AF11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1757,"ΤΕΜ",1,"MC",1,"1FK22045AF110MA0"]
["1FK2204-5AF11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1757,"ΤΕΜ",1,"MC",1,"1FK22045AF110MB0"]
["1FK2204-5AF11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1436,"ΤΕΜ",1,"MC",1,"1FK22045AF110SA0"]
["1FK2204-5AF11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1436,"ΤΕΜ",1,"MC",1,"1FK22045AF110SB0"]
["1FK2204-5AF11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1757,"ΤΕΜ",1,"MC",1,"1FK22045AF111MA0"]
["1FK2204-5AF11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1757,"ΤΕΜ",1,"MC",1,"1FK22045AF111MB0"]
["1FK2204-5AF11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1436,"ΤΕΜ",1,"MC",1,"1FK22045AF111SA0"]
["1FK2204-5AF11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480 V); PN = 0.375 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1436,"ΤΕΜ",1,"MC",1,"1FK22045AF111SB0"]
["1FK2204-5AF11-2MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1757,"ΤΕΜ",1,"MC",1,"1FK22045AF112MA0"]
["1FK2204-5AF11-2MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1757,"ΤΕΜ",1,"MC",1,"1FK22045AF112MB0"]
["1FK2204-5AF11-2SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1436,"ΤΕΜ",1,"MC",1,"1FK22045AF112SA0"]
["1FK2204-5AF11-2SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.75 kW at nN=3000 rpm (380-480V); PN = 0.375 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1436,"ΤΕΜ",1,"MC",1,"1FK22045AF112SB0"]
["1FK2204-5AK00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1410,"ΤΕΜ",1,"MC",1,"1FK22045AK000MA0"]
["1FK2204-5AK00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1410,"ΤΕΜ",1,"MC",1,"1FK22045AK000MB0"]
["1FK2204-5AK00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1089,"ΤΕΜ",1,"MC",1,"1FK22045AK000SA0"]
["1FK2204-5AK00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1089,"ΤΕΜ",1,"MC",1,"1FK22045AK000SB0"]
["1FK2204-5AK00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1410,"ΤΕΜ",1,"MC",1,"1FK22045AK001MA0"]
["1FK2204-5AK00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1410,"ΤΕΜ",1,"MC",1,"1FK22045AK001MB0"]
["1FK2204-5AK00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1089,"ΤΕΜ",1,"MC",1,"1FK22045AK001SA0"]
["1FK2204-5AK00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1089,"ΤΕΜ",1,"MC",1,"1FK22045AK001SB0"]
["1FK2204-5AK00-2MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1410,"ΤΕΜ",1,"MC",1,"1FK22045AK002MA0"]
["1FK2204-5AK00-2MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1410,"ΤΕΜ",1,"MC",1,"1FK22045AK002MB0"]
["1FK2204-5AK00-2SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1089,"ΤΕΜ",1,"MC",1,"1FK22045AK002SA0"]
["1FK2204-5AK00-2SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1089,"ΤΕΜ",1,"MC",1,"1FK22045AK002SB0"]
["1FK2204-5AK01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1499,"ΤΕΜ",1,"MC",1,"1FK22045AK010MA0"]
["1FK2204-5AK01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1499,"ΤΕΜ",1,"MC",1,"1FK22045AK010MB0"]
["1FK2204-5AK01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1178,"ΤΕΜ",1,"MC",1,"1FK22045AK010SA0"]
["1FK2204-5AK01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1178,"ΤΕΜ",1,"MC",1,"1FK22045AK010SB0"]
["1FK2204-5AK01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1499,"ΤΕΜ",1,"MC",1,"1FK22045AK011MA0"]
["1FK2204-5AK01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1499,"ΤΕΜ",1,"MC",1,"1FK22045AK011MB0"]
["1FK2204-5AK01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1178,"ΤΕΜ",1,"MC",1,"1FK22045AK011SA0"]
["1FK2204-5AK01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1178,"ΤΕΜ",1,"MC",1,"1FK22045AK011SB0"]
["1FK2204-5AK01-2MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1499,"ΤΕΜ",1,"MC",1,"1FK22045AK012MA0"]
["1FK2204-5AK01-2MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Βµs; .",1499,"ΤΕΜ",1,"MC",1,"1FK22045AK012MB0"]
["1FK2204-5AK01-2SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1178,"ΤΕΜ",1,"MC",1,"1FK22045AK012SA0"]
["1FK2204-5AK01-2SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Βµs; .",1178,"ΤΕΜ",1,"MC",1,"1FK22045AK012SB0"]
["1FK2204-5AK10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1667,"ΤΕΜ",1,"MC",1,"1FK22045AK100MA0"]
["1FK2204-5AK10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1667,"ΤΕΜ",1,"MC",1,"1FK22045AK100MB0"]
["1FK2204-5AK10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1346,"ΤΕΜ",1,"MC",1,"1FK22045AK100SA0"]
["1FK2204-5AK10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1346,"ΤΕΜ",1,"MC",1,"1FK22045AK100SB0"]
["1FK2204-5AK10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1667,"ΤΕΜ",1,"MC",1,"1FK22045AK101MA0"]
["1FK2204-5AK10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1667,"ΤΕΜ",1,"MC",1,"1FK22045AK101MB0"]
["1FK2204-5AK10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1346,"ΤΕΜ",1,"MC",1,"1FK22045AK101SA0"]
["1FK2204-5AK10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1346,"ΤΕΜ",1,"MC",1,"1FK22045AK101SB0"]
["1FK2204-5AK10-2MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1667,"ΤΕΜ",1,"MC",1,"1FK22045AK102MA0"]
["1FK2204-5AK10-2MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1667,"ΤΕΜ",1,"MC",1,"1FK22045AK102MB0"]
["1FK2204-5AK10-2SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1346,"ΤΕΜ",1,"MC",1,"1FK22045AK102SA0"]
["1FK2204-5AK10-2SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1346,"ΤΕΜ",1,"MC",1,"1FK22045AK102SB0"]
["1FK2204-5AK11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1757,"ΤΕΜ",1,"MC",1,"1FK22045AK110MA0"]
["1FK2204-5AK11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1757,"ΤΕΜ",1,"MC",1,"1FK22045AK110MB0"]
["1FK2204-5AK11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1436,"ΤΕΜ",1,"MC",1,"1FK22045AK110SA0"]
["1FK2204-5AK11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1436,"ΤΕΜ",1,"MC",1,"1FK22045AK110SB0"]
["1FK2204-5AK11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1757,"ΤΕΜ",1,"MC",1,"1FK22045AK111MA0"]
["1FK2204-5AK11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1757,"ΤΕΜ",1,"MC",1,"1FK22045AK111MB0"]
["1FK2204-5AK11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1436,"ΤΕΜ",1,"MC",1,"1FK22045AK111SA0"]
["1FK2204-5AK11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480 V); PN = 0.75 kW At nN=3000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17; Only for 8 kHz / 62.5 Βµs;",1436,"ΤΕΜ",1,"MC",1,"1FK22045AK111SB0"]
["1FK2204-5AK11-2MA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1757,"ΤΕΜ",1,"MC",1,"1FK22045AK112MA0"]
["1FK2204-5AK11-2MB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Βµs; .",1757,"ΤΕΜ",1,"MC",1,"1FK22045AK112MB0"]
["1FK2204-5AK11-2SA0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1436,"ΤΕΜ",1,"MC",1,"1FK22045AK112SA0"]
["1FK2204-5AK11-2SB0","SIMOTICS S-1FK2 CT servo motor M0=2.4 Nm; PN = 0.57 kW at nN=6000 rpm (380-480V); PN = 0.75 kW at nN=3000 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; only for 8 kHz / 62.5 Βµs; .",1436,"ΤΕΜ",1,"MC",1,"1FK22045AK112SB0"]
["1FK2204-6AF00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1474,"ΤΕΜ",1,"MC",1,"1FK22046AF000MA0"]
["1FK2204-6AF00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1474,"ΤΕΜ",1,"MC",1,"1FK22046AF000MB0"]
["1FK2204-6AF00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1153,"ΤΕΜ",1,"MC",1,"1FK22046AF000SA0"]
["1FK2204-6AF00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1153,"ΤΕΜ",1,"MC",1,"1FK22046AF000SB0"]
["1FK2204-6AF00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1474,"ΤΕΜ",1,"MC",1,"1FK22046AF001MA0"]
["1FK2204-6AF00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1474,"ΤΕΜ",1,"MC",1,"1FK22046AF001MB0"]
["1FK2204-6AF00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1153,"ΤΕΜ",1,"MC",1,"1FK22046AF001SA0"]
["1FK2204-6AF00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1153,"ΤΕΜ",1,"MC",1,"1FK22046AF001SB0"]
["1FK2204-6AF00-2MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1474,"ΤΕΜ",1,"MC",1,"1FK22046AF002MA0"]
["1FK2204-6AF00-2MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1474,"ΤΕΜ",1,"MC",1,"1FK22046AF002MB0"]
["1FK2204-6AF00-2SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1153,"ΤΕΜ",1,"MC",1,"1FK22046AF002SA0"]
["1FK2204-6AF00-2SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1153,"ΤΕΜ",1,"MC",1,"1FK22046AF002SB0"]
["1FK2204-6AF01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1563,"ΤΕΜ",1,"MC",1,"1FK22046AF010MA0"]
["1FK2204-6AF01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1563,"ΤΕΜ",1,"MC",1,"1FK22046AF010MB0"]
["1FK2204-6AF01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1242,"ΤΕΜ",1,"MC",1,"1FK22046AF010SA0"]
["1FK2204-6AF01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1242,"ΤΕΜ",1,"MC",1,"1FK22046AF010SB0"]
["1FK2204-6AF01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1563,"ΤΕΜ",1,"MC",1,"1FK22046AF011MA0"]
["1FK2204-6AF01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1563,"ΤΕΜ",1,"MC",1,"1FK22046AF011MB0"]
["1FK2204-6AF01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1242,"ΤΕΜ",1,"MC",1,"1FK22046AF011SA0"]
["1FK2204-6AF01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1242,"ΤΕΜ",1,"MC",1,"1FK22046AF011SB0"]
["1FK2204-6AF01-2MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1563,"ΤΕΜ",1,"MC",1,"1FK22046AF012MA0"]
["1FK2204-6AF01-2MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1563,"ΤΕΜ",1,"MC",1,"1FK22046AF012MB0"]
["1FK2204-6AF01-2SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1242,"ΤΕΜ",1,"MC",1,"1FK22046AF012SA0"]
["1FK2204-6AF01-2SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1242,"ΤΕΜ",1,"MC",1,"1FK22046AF012SB0"]
["1FK2204-6AF10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1731,"ΤΕΜ",1,"MC",1,"1FK22046AF100MA0"]
["1FK2204-6AF10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1731,"ΤΕΜ",1,"MC",1,"1FK22046AF100MB0"]
["1FK2204-6AF10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1410,"ΤΕΜ",1,"MC",1,"1FK22046AF100SA0"]
["1FK2204-6AF10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1410,"ΤΕΜ",1,"MC",1,"1FK22046AF100SB0"]
["1FK2204-6AF10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1731,"ΤΕΜ",1,"MC",1,"1FK22046AF101MA0"]
["1FK2204-6AF10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1731,"ΤΕΜ",1,"MC",1,"1FK22046AF101MB0"]
["1FK2204-6AF10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1410,"ΤΕΜ",1,"MC",1,"1FK22046AF101SA0"]
["1FK2204-6AF10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1410,"ΤΕΜ",1,"MC",1,"1FK22046AF101SB0"]
["1FK2204-6AF10-2MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1731,"ΤΕΜ",1,"MC",1,"1FK22046AF102MA0"]
["1FK2204-6AF10-2MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1731,"ΤΕΜ",1,"MC",1,"1FK22046AF102MB0"]
["1FK2204-6AF10-2SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1410,"ΤΕΜ",1,"MC",1,"1FK22046AF102SA0"]
["1FK2204-6AF10-2SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D14 x 30 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1410,"ΤΕΜ",1,"MC",1,"1FK22046AF102SB0"]
["1FK2204-6AF11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1821,"ΤΕΜ",1,"MC",1,"1FK22046AF110MA0"]
["1FK2204-6AF11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1821,"ΤΕΜ",1,"MC",1,"1FK22046AF110MB0"]
["1FK2204-6AF11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1500,"ΤΕΜ",1,"MC",1,"1FK22046AF110SA0"]
["1FK2204-6AF11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1500,"ΤΕΜ",1,"MC",1,"1FK22046AF110SB0"]
["1FK2204-6AF11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1821,"ΤΕΜ",1,"MC",1,"1FK22046AF111MA0"]
["1FK2204-6AF11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1821,"ΤΕΜ",1,"MC",1,"1FK22046AF111MB0"]
["1FK2204-6AF11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1500,"ΤΕΜ",1,"MC",1,"1FK22046AF111SA0"]
["1FK2204-6AF11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480 V); PN = 0.5 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1500,"ΤΕΜ",1,"MC",1,"1FK22046AF111SB0"]
["1FK2204-6AF11-2MA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with OCC interface; connector size M17, rotatable; .",1821,"ΤΕΜ",1,"MC",1,"1FK22046AF112MA0"]
["1FK2204-6AF11-2MB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder 22-bit + 12-bit multi-turn (encoder AM22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1821,"ΤΕΜ",1,"MC",1,"1FK22046AF112MB0"]
["1FK2204-6AF11-2SA0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with OCC interface; connector size M17, rotatable; .",1500,"ΤΕΜ",1,"MC",1,"1FK22046AF112SA0"]
["1FK2204-6AF11-2SB0","SIMOTICS S-1FK2 CT servo motor M0=3.2 Nm; PN = 1 kW at nN=3000 rpm (380-480V); PN = 0.5 kW at nN=1500 rpm (200-240V); with holding brake; degree of protection IP65; cylindrical shaft D14 x 30 mm; absolute encoder single-turn 22-bit (encoder AS22DQC); with DRIVE-CLiQ plug M17; power connector size M17; .",1500,"ΤΕΜ",1,"MC",1,"1FK22046AF112SB0"]
["1FK2205-2AF00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1497,"ΤΕΜ",1,"MC",1,"1FK22052AF000MA0"]
["1FK2205-2AF00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1497,"ΤΕΜ",1,"MC",1,"1FK22052AF000MB0"]
["1FK2205-2AF00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1176,"ΤΕΜ",1,"MC",1,"1FK22052AF000SA0"]
["1FK2205-2AF00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1176,"ΤΕΜ",1,"MC",1,"1FK22052AF000SB0"]
["1FK2205-2AF00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1497,"ΤΕΜ",1,"MC",1,"1FK22052AF001MA0"]
["1FK2205-2AF00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1497,"ΤΕΜ",1,"MC",1,"1FK22052AF001MB0"]
["1FK2205-2AF00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1176,"ΤΕΜ",1,"MC",1,"1FK22052AF001SA0"]
["1FK2205-2AF00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1176,"ΤΕΜ",1,"MC",1,"1FK22052AF001SB0"]
["1FK2205-2AF01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1586,"ΤΕΜ",1,"MC",1,"1FK22052AF010MA0"]
["1FK2205-2AF01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1586,"ΤΕΜ",1,"MC",1,"1FK22052AF010MB0"]
["1FK2205-2AF01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1265,"ΤΕΜ",1,"MC",1,"1FK22052AF010SA0"]
["1FK2205-2AF01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1265,"ΤΕΜ",1,"MC",1,"1FK22052AF010SB0"]
["1FK2205-2AF01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1586,"ΤΕΜ",1,"MC",1,"1FK22052AF011MA0"]
["1FK2205-2AF01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1586,"ΤΕΜ",1,"MC",1,"1FK22052AF011MB0"]
["1FK2205-2AF01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1265,"ΤΕΜ",1,"MC",1,"1FK22052AF011SA0"]
["1FK2205-2AF01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1265,"ΤΕΜ",1,"MC",1,"1FK22052AF011SB0"]
["1FK2205-2AF10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1797,"ΤΕΜ",1,"MC",1,"1FK22052AF100MA0"]
["1FK2205-2AF10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1797,"ΤΕΜ",1,"MC",1,"1FK22052AF100MB0"]
["1FK2205-2AF10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1476,"ΤΕΜ",1,"MC",1,"1FK22052AF100SA0"]
["1FK2205-2AF10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1476,"ΤΕΜ",1,"MC",1,"1FK22052AF100SB0"]
["1FK2205-2AF10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1797,"ΤΕΜ",1,"MC",1,"1FK22052AF101MA0"]
["1FK2205-2AF10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1797,"ΤΕΜ",1,"MC",1,"1FK22052AF101MB0"]
["1FK2205-2AF10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1476,"ΤΕΜ",1,"MC",1,"1FK22052AF101SA0"]
["1FK2205-2AF10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1476,"ΤΕΜ",1,"MC",1,"1FK22052AF101SB0"]
["1FK2205-2AF11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1887,"ΤΕΜ",1,"MC",1,"1FK22052AF110MA0"]
["1FK2205-2AF11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1887,"ΤΕΜ",1,"MC",1,"1FK22052AF110MB0"]
["1FK2205-2AF11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1566,"ΤΕΜ",1,"MC",1,"1FK22052AF110SA0"]
["1FK2205-2AF11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1566,"ΤΕΜ",1,"MC",1,"1FK22052AF110SB0"]
["1FK2205-2AF11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1887,"ΤΕΜ",1,"MC",1,"1FK22052AF111MA0"]
["1FK2205-2AF11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1887,"ΤΕΜ",1,"MC",1,"1FK22052AF111MB0"]
["1FK2205-2AF11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1566,"ΤΕΜ",1,"MC",1,"1FK22052AF111SA0"]
["1FK2205-2AF11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=3.6 Nm; PN = 0.94 kW at nN=3000 rpm (380-480 V); PN = 0.53 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1566,"ΤΕΜ",1,"MC",1,"1FK22052AF111SB0"]
["1FK2205-4AF00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1708,"ΤΕΜ",1,"MC",1,"1FK22054AF000MA0"]
["1FK2205-4AF00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1708,"ΤΕΜ",1,"MC",1,"1FK22054AF000MB0"]
["1FK2205-4AF00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1387,"ΤΕΜ",1,"MC",1,"1FK22054AF000SA0"]
["1FK2205-4AF00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1387,"ΤΕΜ",1,"MC",1,"1FK22054AF000SB0"]
["1FK2205-4AF00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1708,"ΤΕΜ",1,"MC",1,"1FK22054AF001MA0"]
["1FK2205-4AF00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1708,"ΤΕΜ",1,"MC",1,"1FK22054AF001MB0"]
["1FK2205-4AF00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1387,"ΤΕΜ",1,"MC",1,"1FK22054AF001SA0"]
["1FK2205-4AF00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1387,"ΤΕΜ",1,"MC",1,"1FK22054AF001SB0"]
["1FK2205-4AF01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1798,"ΤΕΜ",1,"MC",1,"1FK22054AF010MA0"]
["1FK2205-4AF01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1798,"ΤΕΜ",1,"MC",1,"1FK22054AF010MB0"]
["1FK2205-4AF01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1477,"ΤΕΜ",1,"MC",1,"1FK22054AF010SA0"]
["1FK2205-4AF01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1477,"ΤΕΜ",1,"MC",1,"1FK22054AF010SB0"]
["1FK2205-4AF01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",1798,"ΤΕΜ",1,"MC",1,"1FK22054AF011MA0"]
["1FK2205-4AF01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1798,"ΤΕΜ",1,"MC",1,"1FK22054AF011MB0"]
["1FK2205-4AF01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1477,"ΤΕΜ",1,"MC",1,"1FK22054AF011SA0"]
["1FK2205-4AF01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1477,"ΤΕΜ",1,"MC",1,"1FK22054AF011SB0"]
["1FK2205-4AF10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",2009,"ΤΕΜ",1,"MC",1,"1FK22054AF100MA0"]
["1FK2205-4AF10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",2009,"ΤΕΜ",1,"MC",1,"1FK22054AF100MB0"]
["1FK2205-4AF10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1688,"ΤΕΜ",1,"MC",1,"1FK22054AF100SA0"]
["1FK2205-4AF10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1688,"ΤΕΜ",1,"MC",1,"1FK22054AF100SB0"]
["1FK2205-4AF10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",2009,"ΤΕΜ",1,"MC",1,"1FK22054AF101MA0"]
["1FK2205-4AF10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",2009,"ΤΕΜ",1,"MC",1,"1FK22054AF101MB0"]
["1FK2205-4AF10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1688,"ΤΕΜ",1,"MC",1,"1FK22054AF101SA0"]
["1FK2205-4AF10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1688,"ΤΕΜ",1,"MC",1,"1FK22054AF101SB0"]
["1FK2205-4AF11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",2098,"ΤΕΜ",1,"MC",1,"1FK22054AF110MA0"]
["1FK2205-4AF11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",2098,"ΤΕΜ",1,"MC",1,"1FK22054AF110MB0"]
["1FK2205-4AF11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1777,"ΤΕΜ",1,"MC",1,"1FK22054AF110SA0"]
["1FK2205-4AF11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D19x40 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1777,"ΤΕΜ",1,"MC",1,"1FK22054AF110SB0"]
["1FK2205-4AF11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M17, rotatable;",2098,"ΤΕΜ",1,"MC",1,"1FK22054AF111MA0"]
["1FK2205-4AF11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",2098,"ΤΕΜ",1,"MC",1,"1FK22054AF111MB0"]
["1FK2205-4AF11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M17, rotatable;",1777,"ΤΕΜ",1,"MC",1,"1FK22054AF111SA0"]
["1FK2205-4AF11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=6 Nm; PN = 1.45 kW at nN=3000 rpm (380-480 V); PN = 0.86 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D19x40 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M17;",1777,"ΤΕΜ",1,"MC",1,"1FK22054AF111SB0"]
["1FK2206-2AF00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",1747,"ΤΕΜ",1,"MC",1,"1FK22062AF000MA0"]
["1FK2206-2AF00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1747,"ΤΕΜ",1,"MC",1,"1FK22062AF000MB0"]
["1FK2206-2AF00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1426,"ΤΕΜ",1,"MC",1,"1FK22062AF000SA0"]
["1FK2206-2AF00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1426,"ΤΕΜ",1,"MC",1,"1FK22062AF000SB0"]
["1FK2206-2AF00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",1747,"ΤΕΜ",1,"MC",1,"1FK22062AF001MA0"]
["1FK2206-2AF00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1747,"ΤΕΜ",1,"MC",1,"1FK22062AF001MB0"]
["1FK2206-2AF00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1426,"ΤΕΜ",1,"MC",1,"1FK22062AF001SA0"]
["1FK2206-2AF00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1426,"ΤΕΜ",1,"MC",1,"1FK22062AF001SB0"]
["1FK2206-2AF01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",1837,"ΤΕΜ",1,"MC",1,"1FK22062AF010MA0"]
["1FK2206-2AF01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1837,"ΤΕΜ",1,"MC",1,"1FK22062AF010MB0"]
["1FK2206-2AF01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1516,"ΤΕΜ",1,"MC",1,"1FK22062AF010SA0"]
["1FK2206-2AF01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1516,"ΤΕΜ",1,"MC",1,"1FK22062AF010SB0"]
["1FK2206-2AF01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",1837,"ΤΕΜ",1,"MC",1,"1FK22062AF011MA0"]
["1FK2206-2AF01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1837,"ΤΕΜ",1,"MC",1,"1FK22062AF011MB0"]
["1FK2206-2AF01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1516,"ΤΕΜ",1,"MC",1,"1FK22062AF011SA0"]
["1FK2206-2AF01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1516,"ΤΕΜ",1,"MC",1,"1FK22062AF011SB0"]
["1FK2206-2AF10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2091,"ΤΕΜ",1,"MC",1,"1FK22062AF100MA0"]
["1FK2206-2AF10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2091,"ΤΕΜ",1,"MC",1,"1FK22062AF100MB0"]
["1FK2206-2AF10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1770,"ΤΕΜ",1,"MC",1,"1FK22062AF100SA0"]
["1FK2206-2AF10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1770,"ΤΕΜ",1,"MC",1,"1FK22062AF100SB0"]
["1FK2206-2AF10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2091,"ΤΕΜ",1,"MC",1,"1FK22062AF101MA0"]
["1FK2206-2AF10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2091,"ΤΕΜ",1,"MC",1,"1FK22062AF101MB0"]
["1FK2206-2AF10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1770,"ΤΕΜ",1,"MC",1,"1FK22062AF101SA0"]
["1FK2206-2AF10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1770,"ΤΕΜ",1,"MC",1,"1FK22062AF101SB0"]
["1FK2206-2AF11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2180,"ΤΕΜ",1,"MC",1,"1FK22062AF110MA0"]
["1FK2206-2AF11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2180,"ΤΕΜ",1,"MC",1,"1FK22062AF110MB0"]
["1FK2206-2AF11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1859,"ΤΕΜ",1,"MC",1,"1FK22062AF110SA0"]
["1FK2206-2AF11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1859,"ΤΕΜ",1,"MC",1,"1FK22062AF110SB0"]
["1FK2206-2AF11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2180,"ΤΕΜ",1,"MC",1,"1FK22062AF111MA0"]
["1FK2206-2AF11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2180,"ΤΕΜ",1,"MC",1,"1FK22062AF111MB0"]
["1FK2206-2AF11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1859,"ΤΕΜ",1,"MC",1,"1FK22062AF111SA0"]
["1FK2206-2AF11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=6.5 Nm; PN = 1.71 kW at nN=3000 rpm (380-480 V); PN = 0.97 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1859,"ΤΕΜ",1,"MC",1,"1FK22062AF111SB0"]
["1FK2206-4AF00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2178,"ΤΕΜ",1,"MC",1,"1FK22064AF000MA0"]
["1FK2206-4AF00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2178,"ΤΕΜ",1,"MC",1,"1FK22064AF000MB0"]
["1FK2206-4AF00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1857,"ΤΕΜ",1,"MC",1,"1FK22064AF000SA0"]
["1FK2206-4AF00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1857,"ΤΕΜ",1,"MC",1,"1FK22064AF000SB0"]
["1FK2206-4AF00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2178,"ΤΕΜ",1,"MC",1,"1FK22064AF001MA0"]
["1FK2206-4AF00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2178,"ΤΕΜ",1,"MC",1,"1FK22064AF001MB0"]
["1FK2206-4AF00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1857,"ΤΕΜ",1,"MC",1,"1FK22064AF001SA0"]
["1FK2206-4AF00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1857,"ΤΕΜ",1,"MC",1,"1FK22064AF001SB0"]
["1FK2206-4AF01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2267,"ΤΕΜ",1,"MC",1,"1FK22064AF010MA0"]
["1FK2206-4AF01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2267,"ΤΕΜ",1,"MC",1,"1FK22064AF010MB0"]
["1FK2206-4AF01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1946,"ΤΕΜ",1,"MC",1,"1FK22064AF010SA0"]
["1FK2206-4AF01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1946,"ΤΕΜ",1,"MC",1,"1FK22064AF010SB0"]
["1FK2206-4AF01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2267,"ΤΕΜ",1,"MC",1,"1FK22064AF011MA0"]
["1FK2206-4AF01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2267,"ΤΕΜ",1,"MC",1,"1FK22064AF011MB0"]
["1FK2206-4AF01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",1946,"ΤΕΜ",1,"MC",1,"1FK22064AF011SA0"]
["1FK2206-4AF01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1946,"ΤΕΜ",1,"MC",1,"1FK22064AF011SB0"]
["1FK2206-4AF10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2521,"ΤΕΜ",1,"MC",1,"1FK22064AF100MA0"]
["1FK2206-4AF10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2521,"ΤΕΜ",1,"MC",1,"1FK22064AF100MB0"]
["1FK2206-4AF10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2200,"ΤΕΜ",1,"MC",1,"1FK22064AF100SA0"]
["1FK2206-4AF10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2200,"ΤΕΜ",1,"MC",1,"1FK22064AF100SB0"]
["1FK2206-4AF10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2521,"ΤΕΜ",1,"MC",1,"1FK22064AF101MA0"]
["1FK2206-4AF10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2521,"ΤΕΜ",1,"MC",1,"1FK22064AF101MB0"]
["1FK2206-4AF10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2200,"ΤΕΜ",1,"MC",1,"1FK22064AF101SA0"]
["1FK2206-4AF10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2200,"ΤΕΜ",1,"MC",1,"1FK22064AF101SB0"]
["1FK2206-4AF11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2611,"ΤΕΜ",1,"MC",1,"1FK22064AF110MA0"]
["1FK2206-4AF11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2611,"ΤΕΜ",1,"MC",1,"1FK22064AF110MB0"]
["1FK2206-4AF11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2289,"ΤΕΜ",1,"MC",1,"1FK22064AF110SA0"]
["1FK2206-4AF11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2289,"ΤΕΜ",1,"MC",1,"1FK22064AF110SB0"]
["1FK2206-4AF11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2611,"ΤΕΜ",1,"MC",1,"1FK22064AF111MA0"]
["1FK2206-4AF11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2611,"ΤΕΜ",1,"MC",1,"1FK22064AF111MB0"]
["1FK2206-4AF11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2289,"ΤΕΜ",1,"MC",1,"1FK22064AF111SA0"]
["1FK2206-4AF11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=12 Nm; PN = 2.85 kW at nN=3000 rpm (380-480 V); PN = 1.72 kW at nN=1500 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2289,"ΤΕΜ",1,"MC",1,"1FK22064AF111SB0"]
["1FK2208-3AC00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2552,"ΤΕΜ",1,"MC",1,"1FK22083AC000MA0"]
["1FK2208-3AC00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2552,"ΤΕΜ",1,"MC",1,"1FK22083AC000MB0"]
["1FK2208-3AC00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2231,"ΤΕΜ",1,"MC",1,"1FK22083AC000SA0"]
["1FK2208-3AC00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2231,"ΤΕΜ",1,"MC",1,"1FK22083AC000SB0"]
["1FK2208-3AC00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2552,"ΤΕΜ",1,"MC",1,"1FK22083AC001MA0"]
["1FK2208-3AC00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2552,"ΤΕΜ",1,"MC",1,"1FK22083AC001MB0"]
["1FK2208-3AC00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2231,"ΤΕΜ",1,"MC",1,"1FK22083AC001SA0"]
["1FK2208-3AC00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2231,"ΤΕΜ",1,"MC",1,"1FK22083AC001SB0"]
["1FK2208-3AC01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2642,"ΤΕΜ",1,"MC",1,"1FK22083AC010MA0"]
["1FK2208-3AC01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2642,"ΤΕΜ",1,"MC",1,"1FK22083AC010MB0"]
["1FK2208-3AC01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2321,"ΤΕΜ",1,"MC",1,"1FK22083AC010SA0"]
["1FK2208-3AC01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2321,"ΤΕΜ",1,"MC",1,"1FK22083AC010SB0"]
["1FK2208-3AC01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2642,"ΤΕΜ",1,"MC",1,"1FK22083AC011MA0"]
["1FK2208-3AC01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2642,"ΤΕΜ",1,"MC",1,"1FK22083AC011MB0"]
["1FK2208-3AC01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2321,"ΤΕΜ",1,"MC",1,"1FK22083AC011SA0"]
["1FK2208-3AC01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2321,"ΤΕΜ",1,"MC",1,"1FK22083AC011SB0"]
["1FK2208-3AC10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2981,"ΤΕΜ",1,"MC",1,"1FK22083AC100MA0"]
["1FK2208-3AC10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2981,"ΤΕΜ",1,"MC",1,"1FK22083AC100MB0"]
["1FK2208-3AC10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2660,"ΤΕΜ",1,"MC",1,"1FK22083AC100SA0"]
["1FK2208-3AC10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2660,"ΤΕΜ",1,"MC",1,"1FK22083AC100SB0"]
["1FK2208-3AC10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2981,"ΤΕΜ",1,"MC",1,"1FK22083AC101MA0"]
["1FK2208-3AC10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2981,"ΤΕΜ",1,"MC",1,"1FK22083AC101MB0"]
["1FK2208-3AC10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2660,"ΤΕΜ",1,"MC",1,"1FK22083AC101SA0"]
["1FK2208-3AC10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2660,"ΤΕΜ",1,"MC",1,"1FK22083AC101SB0"]
["1FK2208-3AC11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3071,"ΤΕΜ",1,"MC",1,"1FK22083AC110MA0"]
["1FK2208-3AC11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3071,"ΤΕΜ",1,"MC",1,"1FK22083AC110MB0"]
["1FK2208-3AC11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2750,"ΤΕΜ",1,"MC",1,"1FK22083AC110SA0"]
["1FK2208-3AC11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2750,"ΤΕΜ",1,"MC",1,"1FK22083AC110SB0"]
["1FK2208-3AC11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3071,"ΤΕΜ",1,"MC",1,"1FK22083AC111MA0"]
["1FK2208-3AC11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3071,"ΤΕΜ",1,"MC",1,"1FK22083AC111MB0"]
["1FK2208-3AC11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2750,"ΤΕΜ",1,"MC",1,"1FK22083AC111SA0"]
["1FK2208-3AC11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=18 Nm; PN = 3.05 kW at nN=2000 rpm (380-480 V); PN = 1.74 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2750,"ΤΕΜ",1,"MC",1,"1FK22083AC111SB0"]
["1FK2208-4AC00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2808,"ΤΕΜ",1,"MC",1,"1FK22084AC000MA0"]
["1FK2208-4AC00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2808,"ΤΕΜ",1,"MC",1,"1FK22084AC000MB0"]
["1FK2208-4AC00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2487,"ΤΕΜ",1,"MC",1,"1FK22084AC000SA0"]
["1FK2208-4AC00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2487,"ΤΕΜ",1,"MC",1,"1FK22084AC000SB0"]
["1FK2208-4AC00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2808,"ΤΕΜ",1,"MC",1,"1FK22084AC001MA0"]
["1FK2208-4AC00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2808,"ΤΕΜ",1,"MC",1,"1FK22084AC001MB0"]
["1FK2208-4AC00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2487,"ΤΕΜ",1,"MC",1,"1FK22084AC001SA0"]
["1FK2208-4AC00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2487,"ΤΕΜ",1,"MC",1,"1FK22084AC001SB0"]
["1FK2208-4AC01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2897,"ΤΕΜ",1,"MC",1,"1FK22084AC010MA0"]
["1FK2208-4AC01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2897,"ΤΕΜ",1,"MC",1,"1FK22084AC010MB0"]
["1FK2208-4AC01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2576,"ΤΕΜ",1,"MC",1,"1FK22084AC010SA0"]
["1FK2208-4AC01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2576,"ΤΕΜ",1,"MC",1,"1FK22084AC010SB0"]
["1FK2208-4AC01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",2897,"ΤΕΜ",1,"MC",1,"1FK22084AC011MA0"]
["1FK2208-4AC01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2897,"ΤΕΜ",1,"MC",1,"1FK22084AC011MB0"]
["1FK2208-4AC01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2576,"ΤΕΜ",1,"MC",1,"1FK22084AC011SA0"]
["1FK2208-4AC01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2576,"ΤΕΜ",1,"MC",1,"1FK22084AC011SB0"]
["1FK2208-4AC10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3237,"ΤΕΜ",1,"MC",1,"1FK22084AC100MA0"]
["1FK2208-4AC10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3237,"ΤΕΜ",1,"MC",1,"1FK22084AC100MB0"]
["1FK2208-4AC10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2916,"ΤΕΜ",1,"MC",1,"1FK22084AC100SA0"]
["1FK2208-4AC10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2916,"ΤΕΜ",1,"MC",1,"1FK22084AC100SB0"]
["1FK2208-4AC10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3237,"ΤΕΜ",1,"MC",1,"1FK22084AC101MA0"]
["1FK2208-4AC10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3237,"ΤΕΜ",1,"MC",1,"1FK22084AC101MB0"]
["1FK2208-4AC10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2916,"ΤΕΜ",1,"MC",1,"1FK22084AC101SA0"]
["1FK2208-4AC10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2916,"ΤΕΜ",1,"MC",1,"1FK22084AC101SB0"]
["1FK2208-4AC11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3326,"ΤΕΜ",1,"MC",1,"1FK22084AC110MA0"]
["1FK2208-4AC11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3326,"ΤΕΜ",1,"MC",1,"1FK22084AC110MB0"]
["1FK2208-4AC11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3005,"ΤΕΜ",1,"MC",1,"1FK22084AC110SA0"]
["1FK2208-4AC11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3005,"ΤΕΜ",1,"MC",1,"1FK22084AC110SB0"]
["1FK2208-4AC11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3326,"ΤΕΜ",1,"MC",1,"1FK22084AC111MA0"]
["1FK2208-4AC11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3326,"ΤΕΜ",1,"MC",1,"1FK22084AC111MB0"]
["1FK2208-4AC11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3005,"ΤΕΜ",1,"MC",1,"1FK22084AC111SA0"]
["1FK2208-4AC11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=22 Nm; PN = 3.55 kW at nN=2000 rpm (380-480 V); PN = 2.15 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3005,"ΤΕΜ",1,"MC",1,"1FK22084AC111SB0"]
["1FK2208-5AC00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3129,"ΤΕΜ",1,"MC",1,"1FK22085AC000MA0"]
["1FK2208-5AC00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3129,"ΤΕΜ",1,"MC",1,"1FK22085AC000MB0"]
["1FK2208-5AC00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2808,"ΤΕΜ",1,"MC",1,"1FK22085AC000SA0"]
["1FK2208-5AC00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2808,"ΤΕΜ",1,"MC",1,"1FK22085AC000SB0"]
["1FK2208-5AC00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3129,"ΤΕΜ",1,"MC",1,"1FK22085AC001MA0"]
["1FK2208-5AC00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3129,"ΤΕΜ",1,"MC",1,"1FK22085AC001MB0"]
["1FK2208-5AC00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2808,"ΤΕΜ",1,"MC",1,"1FK22085AC001SA0"]
["1FK2208-5AC00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2808,"ΤΕΜ",1,"MC",1,"1FK22085AC001SB0"]
["1FK2208-5AC01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3218,"ΤΕΜ",1,"MC",1,"1FK22085AC010MA0"]
["1FK2208-5AC01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3218,"ΤΕΜ",1,"MC",1,"1FK22085AC010MB0"]
["1FK2208-5AC01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2897,"ΤΕΜ",1,"MC",1,"1FK22085AC010SA0"]
["1FK2208-5AC01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2897,"ΤΕΜ",1,"MC",1,"1FK22085AC010SB0"]
["1FK2208-5AC01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3218,"ΤΕΜ",1,"MC",1,"1FK22085AC011MA0"]
["1FK2208-5AC01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3218,"ΤΕΜ",1,"MC",1,"1FK22085AC011MB0"]
["1FK2208-5AC01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2897,"ΤΕΜ",1,"MC",1,"1FK22085AC011SA0"]
["1FK2208-5AC01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2897,"ΤΕΜ",1,"MC",1,"1FK22085AC011SB0"]
["1FK2208-5AC10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3558,"ΤΕΜ",1,"MC",1,"1FK22085AC100MA0"]
["1FK2208-5AC10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3558,"ΤΕΜ",1,"MC",1,"1FK22085AC100MB0"]
["1FK2208-5AC10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3237,"ΤΕΜ",1,"MC",1,"1FK22085AC100SA0"]
["1FK2208-5AC10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3237,"ΤΕΜ",1,"MC",1,"1FK22085AC100SB0"]
["1FK2208-5AC10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3558,"ΤΕΜ",1,"MC",1,"1FK22085AC101MA0"]
["1FK2208-5AC10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3558,"ΤΕΜ",1,"MC",1,"1FK22085AC101MB0"]
["1FK2208-5AC10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3237,"ΤΕΜ",1,"MC",1,"1FK22085AC101SA0"]
["1FK2208-5AC10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3237,"ΤΕΜ",1,"MC",1,"1FK22085AC101SB0"]
["1FK2208-5AC11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3647,"ΤΕΜ",1,"MC",1,"1FK22085AC110MA0"]
["1FK2208-5AC11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3647,"ΤΕΜ",1,"MC",1,"1FK22085AC110MB0"]
["1FK2208-5AC11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3326,"ΤΕΜ",1,"MC",1,"1FK22085AC110SA0"]
["1FK2208-5AC11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3326,"ΤΕΜ",1,"MC",1,"1FK22085AC110SB0"]
["1FK2208-5AC11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3647,"ΤΕΜ",1,"MC",1,"1FK22085AC111MA0"]
["1FK2208-5AC11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3647,"ΤΕΜ",1,"MC",1,"1FK22085AC111MB0"]
["1FK2208-5AC11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3326,"ΤΕΜ",1,"MC",1,"1FK22085AC111SA0"]
["1FK2208-5AC11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=27 Nm; PN = 4 kW at nN=2000 rpm (380-480 V); PN = 2.5 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3326,"ΤΕΜ",1,"MC",1,"1FK22085AC111SB0"]
["1FK2210-3AB00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3300,"ΤΕΜ",1,"MC",1,"1FK22103AB000MA0"]
["1FK2210-3AB00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3300,"ΤΕΜ",1,"MC",1,"1FK22103AB000MB0"]
["1FK2210-3AB00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2979,"ΤΕΜ",1,"MC",1,"1FK22103AB000SA0"]
["1FK2210-3AB00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2979,"ΤΕΜ",1,"MC",1,"1FK22103AB000SB0"]
["1FK2210-3AB00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3300,"ΤΕΜ",1,"MC",1,"1FK22103AB001MA0"]
["1FK2210-3AB00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3300,"ΤΕΜ",1,"MC",1,"1FK22103AB001MB0"]
["1FK2210-3AB00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2979,"ΤΕΜ",1,"MC",1,"1FK22103AB001SA0"]
["1FK2210-3AB00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2979,"ΤΕΜ",1,"MC",1,"1FK22103AB001SB0"]
["1FK2210-3AB01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3390,"ΤΕΜ",1,"MC",1,"1FK22103AB010MA0"]
["1FK2210-3AB01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3390,"ΤΕΜ",1,"MC",1,"1FK22103AB010MB0"]
["1FK2210-3AB01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3069,"ΤΕΜ",1,"MC",1,"1FK22103AB010SA0"]
["1FK2210-3AB01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3069,"ΤΕΜ",1,"MC",1,"1FK22103AB010SB0"]
["1FK2210-3AB01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3390,"ΤΕΜ",1,"MC",1,"1FK22103AB011MA0"]
["1FK2210-3AB01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3390,"ΤΕΜ",1,"MC",1,"1FK22103AB011MB0"]
["1FK2210-3AB01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3069,"ΤΕΜ",1,"MC",1,"1FK22103AB011SA0"]
["1FK2210-3AB01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3069,"ΤΕΜ",1,"MC",1,"1FK22103AB011SB0"]
["1FK2210-3AB10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3772,"ΤΕΜ",1,"MC",1,"1FK22103AB100MA0"]
["1FK2210-3AB10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3772,"ΤΕΜ",1,"MC",1,"1FK22103AB100MB0"]
["1FK2210-3AB10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3451,"ΤΕΜ",1,"MC",1,"1FK22103AB100SA0"]
["1FK2210-3AB10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3451,"ΤΕΜ",1,"MC",1,"1FK22103AB100SB0"]
["1FK2210-3AB10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3772,"ΤΕΜ",1,"MC",1,"1FK22103AB101MA0"]
["1FK2210-3AB10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3772,"ΤΕΜ",1,"MC",1,"1FK22103AB101MB0"]
["1FK2210-3AB10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3451,"ΤΕΜ",1,"MC",1,"1FK22103AB101SA0"]
["1FK2210-3AB10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3451,"ΤΕΜ",1,"MC",1,"1FK22103AB101SB0"]
["1FK2210-3AB11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3862,"ΤΕΜ",1,"MC",1,"1FK22103AB110MA0"]
["1FK2210-3AB11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3862,"ΤΕΜ",1,"MC",1,"1FK22103AB110MB0"]
["1FK2210-3AB11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3540,"ΤΕΜ",1,"MC",1,"1FK22103AB110SA0"]
["1FK2210-3AB11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3540,"ΤΕΜ",1,"MC",1,"1FK22103AB110SB0"]
["1FK2210-3AB11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3862,"ΤΕΜ",1,"MC",1,"1FK22103AB111MA0"]
["1FK2210-3AB11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3862,"ΤΕΜ",1,"MC",1,"1FK22103AB111MB0"]
["1FK2210-3AB11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3540,"ΤΕΜ",1,"MC",1,"1FK22103AB111SA0"]
["1FK2210-3AB11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 4.5 kW at nN=1500 rpm (380-480 V); PN = 2.5 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3540,"ΤΕΜ",1,"MC",1,"1FK22103AB111SB0"]
["1FK2210-3AC00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3300,"ΤΕΜ",1,"MC",1,"1FK22103AC000MA0"]
["1FK2210-3AC00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3300,"ΤΕΜ",1,"MC",1,"1FK22103AC000MB0"]
["1FK2210-3AC00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2979,"ΤΕΜ",1,"MC",1,"1FK22103AC000SA0"]
["1FK2210-3AC00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2979,"ΤΕΜ",1,"MC",1,"1FK22103AC000SB0"]
["1FK2210-3AC00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3300,"ΤΕΜ",1,"MC",1,"1FK22103AC001MA0"]
["1FK2210-3AC00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3300,"ΤΕΜ",1,"MC",1,"1FK22103AC001MB0"]
["1FK2210-3AC00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",2979,"ΤΕΜ",1,"MC",1,"1FK22103AC001SA0"]
["1FK2210-3AC00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2979,"ΤΕΜ",1,"MC",1,"1FK22103AC001SB0"]
["1FK2210-3AC01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3390,"ΤΕΜ",1,"MC",1,"1FK22103AC010MA0"]
["1FK2210-3AC01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3390,"ΤΕΜ",1,"MC",1,"1FK22103AC010MB0"]
["1FK2210-3AC01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3069,"ΤΕΜ",1,"MC",1,"1FK22103AC010SA0"]
["1FK2210-3AC01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3069,"ΤΕΜ",1,"MC",1,"1FK22103AC010SB0"]
["1FK2210-3AC01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3390,"ΤΕΜ",1,"MC",1,"1FK22103AC011MA0"]
["1FK2210-3AC01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3390,"ΤΕΜ",1,"MC",1,"1FK22103AC011MB0"]
["1FK2210-3AC01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3069,"ΤΕΜ",1,"MC",1,"1FK22103AC011SA0"]
["1FK2210-3AC01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3069,"ΤΕΜ",1,"MC",1,"1FK22103AC011SB0"]
["1FK2210-3AC10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3772,"ΤΕΜ",1,"MC",1,"1FK22103AC100MA0"]
["1FK2210-3AC10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3772,"ΤΕΜ",1,"MC",1,"1FK22103AC100MB0"]
["1FK2210-3AC10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3451,"ΤΕΜ",1,"MC",1,"1FK22103AC100SA0"]
["1FK2210-3AC10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3451,"ΤΕΜ",1,"MC",1,"1FK22103AC100SB0"]
["1FK2210-3AC10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3772,"ΤΕΜ",1,"MC",1,"1FK22103AC101MA0"]
["1FK2210-3AC10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3772,"ΤΕΜ",1,"MC",1,"1FK22103AC101MB0"]
["1FK2210-3AC10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3451,"ΤΕΜ",1,"MC",1,"1FK22103AC101SA0"]
["1FK2210-3AC10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3451,"ΤΕΜ",1,"MC",1,"1FK22103AC101SB0"]
["1FK2210-3AC11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3862,"ΤΕΜ",1,"MC",1,"1FK22103AC110MA0"]
["1FK2210-3AC11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3862,"ΤΕΜ",1,"MC",1,"1FK22103AC110MB0"]
["1FK2210-3AC11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3540,"ΤΕΜ",1,"MC",1,"1FK22103AC110SA0"]
["1FK2210-3AC11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3540,"ΤΕΜ",1,"MC",1,"1FK22103AC110SB0"]
["1FK2210-3AC11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3862,"ΤΕΜ",1,"MC",1,"1FK22103AC111MA0"]
["1FK2210-3AC11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3862,"ΤΕΜ",1,"MC",1,"1FK22103AC111MB0"]
["1FK2210-3AC11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3540,"ΤΕΜ",1,"MC",1,"1FK22103AC111SA0"]
["1FK2210-3AC11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=30 Nm; PN = 5.5 kW at nN=2000 rpm (380-480 V); PN = 3.2 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3540,"ΤΕΜ",1,"MC",1,"1FK22103AC111SB0"]
["1FK2210-4AB00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3968,"ΤΕΜ",1,"MC",1,"1FK22104AB000MA0"]
["1FK2210-4AB00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3968,"ΤΕΜ",1,"MC",1,"1FK22104AB000MB0"]
["1FK2210-4AB00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3647,"ΤΕΜ",1,"MC",1,"1FK22104AB000SA0"]
["1FK2210-4AB00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3647,"ΤΕΜ",1,"MC",1,"1FK22104AB000SB0"]
["1FK2210-4AB00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3968,"ΤΕΜ",1,"MC",1,"1FK22104AB001MA0"]
["1FK2210-4AB00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3968,"ΤΕΜ",1,"MC",1,"1FK22104AB001MB0"]
["1FK2210-4AB00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3647,"ΤΕΜ",1,"MC",1,"1FK22104AB001SA0"]
["1FK2210-4AB00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3647,"ΤΕΜ",1,"MC",1,"1FK22104AB001SB0"]
["1FK2210-4AB01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",4058,"ΤΕΜ",1,"MC",1,"1FK22104AB010MA0"]
["1FK2210-4AB01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4058,"ΤΕΜ",1,"MC",1,"1FK22104AB010MB0"]
["1FK2210-4AB01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3737,"ΤΕΜ",1,"MC",1,"1FK22104AB010SA0"]
["1FK2210-4AB01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3737,"ΤΕΜ",1,"MC",1,"1FK22104AB010SB0"]
["1FK2210-4AB01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",4058,"ΤΕΜ",1,"MC",1,"1FK22104AB011MA0"]
["1FK2210-4AB01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4058,"ΤΕΜ",1,"MC",1,"1FK22104AB011MB0"]
["1FK2210-4AB01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3737,"ΤΕΜ",1,"MC",1,"1FK22104AB011SA0"]
["1FK2210-4AB01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3737,"ΤΕΜ",1,"MC",1,"1FK22104AB011SB0"]
["1FK2210-4AB10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",4439,"ΤΕΜ",1,"MC",1,"1FK22104AB100MA0"]
["1FK2210-4AB10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4439,"ΤΕΜ",1,"MC",1,"1FK22104AB100MB0"]
["1FK2210-4AB10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",4118,"ΤΕΜ",1,"MC",1,"1FK22104AB100SA0"]
["1FK2210-4AB10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4118,"ΤΕΜ",1,"MC",1,"1FK22104AB100SB0"]
["1FK2210-4AB10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",4439,"ΤΕΜ",1,"MC",1,"1FK22104AB101MA0"]
["1FK2210-4AB10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4439,"ΤΕΜ",1,"MC",1,"1FK22104AB101MB0"]
["1FK2210-4AB10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",4118,"ΤΕΜ",1,"MC",1,"1FK22104AB101SA0"]
["1FK2210-4AB10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4118,"ΤΕΜ",1,"MC",1,"1FK22104AB101SB0"]
["1FK2210-4AB11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",4529,"ΤΕΜ",1,"MC",1,"1FK22104AB110MA0"]
["1FK2210-4AB11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4529,"ΤΕΜ",1,"MC",1,"1FK22104AB110MB0"]
["1FK2210-4AB11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",4208,"ΤΕΜ",1,"MC",1,"1FK22104AB110SA0"]
["1FK2210-4AB11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4208,"ΤΕΜ",1,"MC",1,"1FK22104AB110SB0"]
["1FK2210-4AB11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",4529,"ΤΕΜ",1,"MC",1,"1FK22104AB111MA0"]
["1FK2210-4AB11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4529,"ΤΕΜ",1,"MC",1,"1FK22104AB111MB0"]
["1FK2210-4AB11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",4208,"ΤΕΜ",1,"MC",1,"1FK22104AB111SA0"]
["1FK2210-4AB11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 5.4 kW at nN=1500 rpm (380-480 V); PN = 3.05 kW at nN=750 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4208,"ΤΕΜ",1,"MC",1,"1FK22104AB111SB0"]
["1FK2210-4AC00-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3968,"ΤΕΜ",1,"MC",1,"1FK22104AC000MA0"]
["1FK2210-4AC00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3968,"ΤΕΜ",1,"MC",1,"1FK22104AC000MB0"]
["1FK2210-4AC00-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3647,"ΤΕΜ",1,"MC",1,"1FK22104AC000SA0"]
["1FK2210-4AC00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3647,"ΤΕΜ",1,"MC",1,"1FK22104AC000SB0"]
["1FK2210-4AC00-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",3968,"ΤΕΜ",1,"MC",1,"1FK22104AC001MA0"]
["1FK2210-4AC00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3968,"ΤΕΜ",1,"MC",1,"1FK22104AC001MB0"]
["1FK2210-4AC00-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3647,"ΤΕΜ",1,"MC",1,"1FK22104AC001SA0"]
["1FK2210-4AC00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3647,"ΤΕΜ",1,"MC",1,"1FK22104AC001SB0"]
["1FK2210-4AC01-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",4058,"ΤΕΜ",1,"MC",1,"1FK22104AC010MA0"]
["1FK2210-4AC01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4058,"ΤΕΜ",1,"MC",1,"1FK22104AC010MB0"]
["1FK2210-4AC01-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3737,"ΤΕΜ",1,"MC",1,"1FK22104AC010SA0"]
["1FK2210-4AC01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3737,"ΤΕΜ",1,"MC",1,"1FK22104AC010SB0"]
["1FK2210-4AC01-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",4058,"ΤΕΜ",1,"MC",1,"1FK22104AC011MA0"]
["1FK2210-4AC01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4058,"ΤΕΜ",1,"MC",1,"1FK22104AC011MB0"]
["1FK2210-4AC01-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",3737,"ΤΕΜ",1,"MC",1,"1FK22104AC011SA0"]
["1FK2210-4AC01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3737,"ΤΕΜ",1,"MC",1,"1FK22104AC011SB0"]
["1FK2210-4AC10-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",4439,"ΤΕΜ",1,"MC",1,"1FK22104AC100MA0"]
["1FK2210-4AC10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4439,"ΤΕΜ",1,"MC",1,"1FK22104AC100MB0"]
["1FK2210-4AC10-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",4118,"ΤΕΜ",1,"MC",1,"1FK22104AC100SA0"]
["1FK2210-4AC10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4118,"ΤΕΜ",1,"MC",1,"1FK22104AC100SB0"]
["1FK2210-4AC10-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",4439,"ΤΕΜ",1,"MC",1,"1FK22104AC101MA0"]
["1FK2210-4AC10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4439,"ΤΕΜ",1,"MC",1,"1FK22104AC101MB0"]
["1FK2210-4AC10-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",4118,"ΤΕΜ",1,"MC",1,"1FK22104AC101SA0"]
["1FK2210-4AC10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4118,"ΤΕΜ",1,"MC",1,"1FK22104AC101SB0"]
["1FK2210-4AC11-0MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",4529,"ΤΕΜ",1,"MC",1,"1FK22104AC110MA0"]
["1FK2210-4AC11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4529,"ΤΕΜ",1,"MC",1,"1FK22104AC110MB0"]
["1FK2210-4AC11-0SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",4208,"ΤΕΜ",1,"MC",1,"1FK22104AC110SA0"]
["1FK2210-4AC11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4208,"ΤΕΜ",1,"MC",1,"1FK22104AC110SB0"]
["1FK2210-4AC11-1MA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With OCC interface; Connector size M23, rotatable;",4529,"ΤΕΜ",1,"MC",1,"1FK22104AC111MA0"]
["1FK2210-4AC11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4529,"ΤΕΜ",1,"MC",1,"1FK22104AC111MB0"]
["1FK2210-4AC11-1SA0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With OCC interface; Connector size M23, rotatable;",4208,"ΤΕΜ",1,"MC",1,"1FK22104AC111SA0"]
["1FK2210-4AC11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=40 Nm; PN = 6.4 kW at nN=2000 rpm (380-480 V); PN = 3.9 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",4208,"ΤΕΜ",1,"MC",1,"1FK22104AC111SB0"]
["1FK2210-5AC00-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4620,"ΤΕΜ",1,"MC",1,"1FK22105AC000MB0"]
["1FK2210-5AC00-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4299,"ΤΕΜ",1,"MC",1,"1FK22105AC000SB0"]
["1FK2210-5AC00-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4620,"ΤΕΜ",1,"MC",1,"1FK22105AC001MB0"]
["1FK2210-5AC00-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4299,"ΤΕΜ",1,"MC",1,"1FK22105AC001SB0"]
["1FK2210-5AC01-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4710,"ΤΕΜ",1,"MC",1,"1FK22105AC010MB0"]
["1FK2210-5AC01-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4389,"ΤΕΜ",1,"MC",1,"1FK22105AC010SB0"]
["1FK2210-5AC01-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4710,"ΤΕΜ",1,"MC",1,"1FK22105AC011MB0"]
["1FK2210-5AC01-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4389,"ΤΕΜ",1,"MC",1,"1FK22105AC011SB0"]
["1FK2210-5AC10-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",5092,"ΤΕΜ",1,"MC",1,"1FK22105AC100MB0"]
["1FK2210-5AC10-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4771,"ΤΕΜ",1,"MC",1,"1FK22105AC100SB0"]
["1FK2210-5AC10-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",5092,"ΤΕΜ",1,"MC",1,"1FK22105AC101MB0"]
["1FK2210-5AC10-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP64; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4771,"ΤΕΜ",1,"MC",1,"1FK22105AC101SB0"]
["1FK2210-5AC11-0MB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",5181,"ΤΕΜ",1,"MC",1,"1FK22105AC110MB0"]
["1FK2210-5AC11-0SB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Cylindrical shaft D38x80 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4860,"ΤΕΜ",1,"MC",1,"1FK22105AC110SB0"]
["1FK2210-5AC11-1MB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",5181,"ΤΕΜ",1,"MC",1,"1FK22105AC111MB0"]
["1FK2210-5AC11-1SB0","SIMOTICS S-1FK2 CT Servo motor M0=50 Nm; PN = 7.1 kW at nN=2000 rpm (380-480 V); PN = 4.55 kW at nN=1000 rpm (200-240 V); With holding brake; Degree of protection IP65; Shaft D38x80 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M40;",4860,"ΤΕΜ",1,"MC",1,"1FK22105AC111SB0"]
["1FK2306-2AC00-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1708,"ΤΕΜ",1,"MC",1,"1FK23062AC000MB0"]
["1FK2306-2AC00-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1387,"ΤΕΜ",1,"MC",1,"1FK23062AC000SB0"]
["1FK2306-2AC00-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1708,"ΤΕΜ",1,"MC",1,"1FK23062AC001MB0"]
["1FK2306-2AC00-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1387,"ΤΕΜ",1,"MC",1,"1FK23062AC001SB0"]
["1FK2306-2AC01-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1798,"ΤΕΜ",1,"MC",1,"1FK23062AC010MB0"]
["1FK2306-2AC01-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1477,"ΤΕΜ",1,"MC",1,"1FK23062AC010SB0"]
["1FK2306-2AC01-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1798,"ΤΕΜ",1,"MC",1,"1FK23062AC011MB0"]
["1FK2306-2AC01-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1477,"ΤΕΜ",1,"MC",1,"1FK23062AC011SB0"]
["1FK2306-2AC10-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2052,"ΤΕΜ",1,"MC",1,"1FK23062AC100MB0"]
["1FK2306-2AC10-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1730,"ΤΕΜ",1,"MC",1,"1FK23062AC100SB0"]
["1FK2306-2AC10-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2052,"ΤΕΜ",1,"MC",1,"1FK23062AC101MB0"]
["1FK2306-2AC10-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1730,"ΤΕΜ",1,"MC",1,"1FK23062AC101SB0"]
["1FK2306-2AC11-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2141,"ΤΕΜ",1,"MC",1,"1FK23062AC110MB0"]
["1FK2306-2AC11-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1820,"ΤΕΜ",1,"MC",1,"1FK23062AC110SB0"]
["1FK2306-2AC11-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2141,"ΤΕΜ",1,"MC",1,"1FK23062AC111MB0"]
["1FK2306-2AC11-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=6 Nm; PN = 1.15 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1820,"ΤΕΜ",1,"MC",1,"1FK23062AC111SB0"]
["1FK2306-4AC00-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2178,"ΤΕΜ",1,"MC",1,"1FK23064AC000MB0"]
["1FK2306-4AC00-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1857,"ΤΕΜ",1,"MC",1,"1FK23064AC000SB0"]
["1FK2306-4AC00-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2178,"ΤΕΜ",1,"MC",1,"1FK23064AC001MB0"]
["1FK2306-4AC00-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1857,"ΤΕΜ",1,"MC",1,"1FK23064AC001SB0"]
["1FK2306-4AC01-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2267,"ΤΕΜ",1,"MC",1,"1FK23064AC010MB0"]
["1FK2306-4AC01-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1946,"ΤΕΜ",1,"MC",1,"1FK23064AC010SB0"]
["1FK2306-4AC01-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2267,"ΤΕΜ",1,"MC",1,"1FK23064AC011MB0"]
["1FK2306-4AC01-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",1946,"ΤΕΜ",1,"MC",1,"1FK23064AC011SB0"]
["1FK2306-4AC10-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2521,"ΤΕΜ",1,"MC",1,"1FK23064AC100MB0"]
["1FK2306-4AC10-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP64; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2200,"ΤΕΜ",1,"MC",1,"1FK23064AC100SB0"]
["1FK2306-4AC10-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2521,"ΤΕΜ",1,"MC",1,"1FK23064AC101MB0"]
["1FK2306-4AC10-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP64; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2200,"ΤΕΜ",1,"MC",1,"1FK23064AC101SB0"]
["1FK2306-4AC11-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2611,"ΤΕΜ",1,"MC",1,"1FK23064AC110MB0"]
["1FK2306-4AC11-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP65; Cylindrical shaft D24x50 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2289,"ΤΕΜ",1,"MC",1,"1FK23064AC110SB0"]
["1FK2306-4AC11-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2611,"ΤΕΜ",1,"MC",1,"1FK23064AC111MB0"]
["1FK2306-4AC11-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=12 Nm; PN = 2.2 kW at nN=2000 rpm (380-480 V); With holding brake; Degree of protection IP65; Shaft D24x50 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2289,"ΤΕΜ",1,"MC",1,"1FK23064AC111SB0"]
["1FK2308-3AB00-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2552,"ΤΕΜ",1,"MC",1,"1FK23083AB000MB0"]
["1FK2308-3AB00-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2231,"ΤΕΜ",1,"MC",1,"1FK23083AB000SB0"]
["1FK2308-3AB00-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2552,"ΤΕΜ",1,"MC",1,"1FK23083AB001MB0"]
["1FK2308-3AB00-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2231,"ΤΕΜ",1,"MC",1,"1FK23083AB001SB0"]
["1FK2308-3AB01-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2642,"ΤΕΜ",1,"MC",1,"1FK23083AB010MB0"]
["1FK2308-3AB01-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2321,"ΤΕΜ",1,"MC",1,"1FK23083AB010SB0"]
["1FK2308-3AB01-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2642,"ΤΕΜ",1,"MC",1,"1FK23083AB011MB0"]
["1FK2308-3AB01-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2321,"ΤΕΜ",1,"MC",1,"1FK23083AB011SB0"]
["1FK2308-3AB10-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2981,"ΤΕΜ",1,"MC",1,"1FK23083AB100MB0"]
["1FK2308-3AB10-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2660,"ΤΕΜ",1,"MC",1,"1FK23083AB100SB0"]
["1FK2308-3AB10-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2981,"ΤΕΜ",1,"MC",1,"1FK23083AB101MB0"]
["1FK2308-3AB10-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2660,"ΤΕΜ",1,"MC",1,"1FK23083AB101SB0"]
["1FK2308-3AB11-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3071,"ΤΕΜ",1,"MC",1,"1FK23083AB110MB0"]
["1FK2308-3AB11-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2750,"ΤΕΜ",1,"MC",1,"1FK23083AB110SB0"]
["1FK2308-3AB11-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3071,"ΤΕΜ",1,"MC",1,"1FK23083AB111MB0"]
["1FK2308-3AB11-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=18 Nm; PN = 2.5 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2750,"ΤΕΜ",1,"MC",1,"1FK23083AB111SB0"]
["1FK2308-4AB00-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2808,"ΤΕΜ",1,"MC",1,"1FK23084AB000MB0"]
["1FK2308-4AB00-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2487,"ΤΕΜ",1,"MC",1,"1FK23084AB000SB0"]
["1FK2308-4AB00-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2808,"ΤΕΜ",1,"MC",1,"1FK23084AB001MB0"]
["1FK2308-4AB00-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2487,"ΤΕΜ",1,"MC",1,"1FK23084AB001SB0"]
["1FK2308-4AB01-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2897,"ΤΕΜ",1,"MC",1,"1FK23084AB010MB0"]
["1FK2308-4AB01-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2576,"ΤΕΜ",1,"MC",1,"1FK23084AB010SB0"]
["1FK2308-4AB01-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2897,"ΤΕΜ",1,"MC",1,"1FK23084AB011MB0"]
["1FK2308-4AB01-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2576,"ΤΕΜ",1,"MC",1,"1FK23084AB011SB0"]
["1FK2308-4AB10-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3237,"ΤΕΜ",1,"MC",1,"1FK23084AB100MB0"]
["1FK2308-4AB10-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP64; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2916,"ΤΕΜ",1,"MC",1,"1FK23084AB100SB0"]
["1FK2308-4AB10-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3237,"ΤΕΜ",1,"MC",1,"1FK23084AB101MB0"]
["1FK2308-4AB10-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP64; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",2916,"ΤΕΜ",1,"MC",1,"1FK23084AB101SB0"]
["1FK2308-4AB11-0MB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3326,"ΤΕΜ",1,"MC",1,"1FK23084AB110MB0"]
["1FK2308-4AB11-0SB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP65; Cylindrical shaft D32x58 mm; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3005,"ΤΕΜ",1,"MC",1,"1FK23084AB110SB0"]
["1FK2308-4AB11-1MB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder 22-bit + 12-bit Multi-turn (encoder AM22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3326,"ΤΕΜ",1,"MC",1,"1FK23084AB111MB0"]
["1FK2308-4AB11-1SB0","SIMOTICS S-1FK2 HI Servo motor M0=22 Nm; PN = 2.9 kW at nN=1500 rpm (380-480 V); With holding brake; Degree of protection IP65; Shaft D32x58 mm with feather key; Absolute encoder single-turn 22-bit (encoder AS22DQC); With DRIVE-CLiQ plug M17; Power connector size M23;",3005,"ΤΕΜ",1,"MC",1,"1FK23084AB111SB0"]
["1FK7011-5AK24-1AA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1506,"ΤΕΜ",1,"MC",1,"1FK70115AK241AA3"]
["1FK7011-5AK24-1AB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1770,"ΤΕΜ",1,"MC",1,"1FK70115AK241AB3"]
["1FK7011-5AK24-1AG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1456,"ΤΕΜ",1,"MC",1,"1FK70115AK241AG3"]
["1FK7011-5AK24-1AH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1663,"ΤΕΜ",1,"MC",1,"1FK70115AK241AH3"]
["1FK7011-5AK24-1JA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1349,"ΤΕΜ",1,"MC",1,"1FK70115AK241JA3"]
["1FK7011-5AK24-1JB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1613,"ΤΕΜ",1,"MC",1,"1FK70115AK241JB3"]
["1FK7011-5AK24-1JG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1298,"ΤΕΜ",1,"MC",1,"1FK70115AK241JG3"]
["1FK7011-5AK24-1JH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1506,"ΤΕΜ",1,"MC",1,"1FK70115AK241JH3"]
["1FK7011-5AK24-1SA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",820,"ΤΕΜ",1,"MC",1,"1FK70115AK241SA3"]
["1FK7011-5AK24-1SB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1084,"ΤΕΜ",1,"MC",1,"1FK70115AK241SB3"]
["1FK7011-5AK24-1SG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",769,"ΤΕΜ",1,"MC",1,"1FK70115AK241SG3"]
["1FK7011-5AK24-1SH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",977,"ΤΕΜ",1,"MC",1,"1FK70115AK241SH3"]
["1FK7011-5AK24-1TA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",820,"ΤΕΜ",1,"MC",1,"1FK70115AK241TA3"]
["1FK7011-5AK24-1TB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1084,"ΤΕΜ",1,"MC",1,"1FK70115AK241TB3"]
["1FK7011-5AK24-1TG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",769,"ΤΕΜ",1,"MC",1,"1FK70115AK241TG3"]
["1FK7011-5AK24-1TH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.18Nm, 100K, 6000rpm 0.05kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",977,"ΤΕΜ",1,"MC",1,"1FK70115AK241TH3"]
["1FK7011-5AK74-1AA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1506,"ΤΕΜ",1,"MC",1,"1FK70115AK741AA3"]
["1FK7011-5AK74-1AB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1770,"ΤΕΜ",1,"MC",1,"1FK70115AK741AB3"]
["1FK7011-5AK74-1AG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1456,"ΤΕΜ",1,"MC",1,"1FK70115AK741AG3"]
["1FK7011-5AK74-1AH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1663,"ΤΕΜ",1,"MC",1,"1FK70115AK741AH3"]
["1FK7011-5AK74-1JA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1349,"ΤΕΜ",1,"MC",1,"1FK70115AK741JA3"]
["1FK7011-5AK74-1JB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1613,"ΤΕΜ",1,"MC",1,"1FK70115AK741JB3"]
["1FK7011-5AK74-1JG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1298,"ΤΕΜ",1,"MC",1,"1FK70115AK741JG3"]
["1FK7011-5AK74-1JH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1506,"ΤΕΜ",1,"MC",1,"1FK70115AK741JH3"]
["1FK7011-5AK74-1SA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",820,"ΤΕΜ",1,"MC",1,"1FK70115AK741SA3"]
["1FK7011-5AK74-1SB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1084,"ΤΕΜ",1,"MC",1,"1FK70115AK741SB3"]
["1FK7011-5AK74-1SG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",769,"ΤΕΜ",1,"MC",1,"1FK70115AK741SG3"]
["1FK7011-5AK74-1SH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",977,"ΤΕΜ",1,"MC",1,"1FK70115AK741SH3"]
["1FK7011-5AK74-1TA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",820,"ΤΕΜ",1,"MC",1,"1FK70115AK741TA3"]
["1FK7011-5AK74-1TB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1084,"ΤΕΜ",1,"MC",1,"1FK70115AK741TB3"]
["1FK7011-5AK74-1TG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",769,"ΤΕΜ",1,"MC",1,"1FK70115AK741TG3"]
["1FK7011-5AK74-1TH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.18Nm, 100K, 6000rpm; 0.05kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",977,"ΤΕΜ",1,"MC",1,"1FK70115AK741TH3"]
["1FK7015-5AK24-1AA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1603,"ΤΕΜ",1,"MC",1,"1FK70155AK241AA3"]
["1FK7015-5AK24-1AB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1867,"ΤΕΜ",1,"MC",1,"1FK70155AK241AB3"]
["1FK7015-5AK24-1AG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1552,"ΤΕΜ",1,"MC",1,"1FK70155AK241AG3"]
["1FK7015-5AK24-1AH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1760,"ΤΕΜ",1,"MC",1,"1FK70155AK241AH3"]
["1FK7015-5AK24-1JA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1446,"ΤΕΜ",1,"MC",1,"1FK70155AK241JA3"]
["1FK7015-5AK24-1JB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1709,"ΤΕΜ",1,"MC",1,"1FK70155AK241JB3"]
["1FK7015-5AK24-1JG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1395,"ΤΕΜ",1,"MC",1,"1FK70155AK241JG3"]
["1FK7015-5AK24-1JH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1603,"ΤΕΜ",1,"MC",1,"1FK70155AK241JH3"]
["1FK7015-5AK24-1SA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",916,"ΤΕΜ",1,"MC",1,"1FK70155AK241SA3"]
["1FK7015-5AK24-1SB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1180,"ΤΕΜ",1,"MC",1,"1FK70155AK241SB3"]
["1FK7015-5AK24-1SG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",866,"ΤΕΜ",1,"MC",1,"1FK70155AK241SG3"]
["1FK7015-5AK24-1SH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1073,"ΤΕΜ",1,"MC",1,"1FK70155AK241SH3"]
["1FK7015-5AK24-1TA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",916,"ΤΕΜ",1,"MC",1,"1FK70155AK241TA3"]
["1FK7015-5AK24-1TB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1180,"ΤΕΜ",1,"MC",1,"1FK70155AK241TB3"]
["1FK7015-5AK24-1TG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",866,"ΤΕΜ",1,"MC",1,"1FK70155AK241TG3"]
["1FK7015-5AK24-1TH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.35Nm, 100K, 6000rpm, 0.10kW Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1073,"ΤΕΜ",1,"MC",1,"1FK70155AK241TH3"]
["1FK7015-5AK74-1AA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1603,"ΤΕΜ",1,"MC",1,"1FK70155AK741AA3"]
["1FK7015-5AK74-1AB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1867,"ΤΕΜ",1,"MC",1,"1FK70155AK741AB3"]
["1FK7015-5AK74-1AG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1552,"ΤΕΜ",1,"MC",1,"1FK70155AK741AG3"]
["1FK7015-5AK74-1AH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1760,"ΤΕΜ",1,"MC",1,"1FK70155AK741AH3"]
["1FK7015-5AK74-1JA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",1446,"ΤΕΜ",1,"MC",1,"1FK70155AK741JA3"]
["1FK7015-5AK74-1JB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1709,"ΤΕΜ",1,"MC",1,"1FK70155AK741JB3"]
["1FK7015-5AK74-1JG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",1395,"ΤΕΜ",1,"MC",1,"1FK70155AK741JG3"]
["1FK7015-5AK74-1JH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1603,"ΤΕΜ",1,"MC",1,"1FK70155AK741JH3"]
["1FK7015-5AK74-1SA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",916,"ΤΕΜ",1,"MC",1,"1FK70155AK741SA3"]
["1FK7015-5AK74-1SB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1180,"ΤΕΜ",1,"MC",1,"1FK70155AK741SB3"]
["1FK7015-5AK74-1SG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",866,"ΤΕΜ",1,"MC",1,"1FK70155AK741SG3"]
["1FK7015-5AK74-1SH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1073,"ΤΕΜ",1,"MC",1,"1FK70155AK741SH3"]
["1FK7015-5AK74-1TA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE",916,"ΤΕΜ",1,"MC",1,"1FK70155AK741TA3"]
["1FK7015-5AK74-1TB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE",1180,"ΤΕΜ",1,"MC",1,"1FK70155AK741TB3"]
["1FK7015-5AK74-1TG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE",866,"ΤΕΜ",1,"MC",1,"1FK70155AK741TG3"]
["1FK7015-5AK74-1TH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.35Nm, 100K, 6000rpm 0.10kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° Degree of protection IP54; paint finish RAL7016 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1073,"ΤΕΜ",1,"MC",1,"1FK70155AK741TH3"]
["1FK7022-5AF04-1AB0","SIMOTICS S-1FK7 Synchronous servo motor 1FK7 Compact; naturally cooled; NN=3000rpm; UDC=24V; IMB 5 design; Power connector rotatable; Incremental encoder sin/cos 1VSS 2048 S/R (encoder I-2048); Shaft with feather key Tolerance N with holding brake; Degree of protection IP64; Customer-specific version customer-specific motor",2107,"ΤΕΜ",1,"MC",1,"1FK70225AF041AB0"]
["1FK7022-5AK21-1DA0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2160,"ΤΕΜ",1,"MC",1,"1FK70225AK211DA0"]
["1FK7022-5AK21-1DA2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2273,"ΤΕΜ",1,"MC",1,"1FK70225AK211DA2"]
["1FK7022-5AK21-1DA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2214,"ΤΕΜ",1,"MC",1,"1FK70225AK211DA3"]
["1FK7022-5AK21-1DA5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2327,"ΤΕΜ",1,"MC",1,"1FK70225AK211DA5"]
["1FK7022-5AK21-1DA8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2448,"ΤΕΜ",1,"MC",1,"1FK70225AK211DA8"]
["1FK7022-5AK21-1DB0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2424,"ΤΕΜ",1,"MC",1,"1FK70225AK211DB0"]
["1FK7022-5AK21-1DB2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2536,"ΤΕΜ",1,"MC",1,"1FK70225AK211DB2"]
["1FK7022-5AK21-1DB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2478,"ΤΕΜ",1,"MC",1,"1FK70225AK211DB3"]
["1FK7022-5AK21-1DB5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2591,"ΤΕΜ",1,"MC",1,"1FK70225AK211DB5"]
["1FK7022-5AK21-1DB8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2711,"ΤΕΜ",1,"MC",1,"1FK70225AK211DB8"]
["1FK7022-5AK21-1DG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2056,"ΤΕΜ",1,"MC",1,"1FK70225AK211DG0"]
["1FK7022-5AK21-1DG2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2169,"ΤΕΜ",1,"MC",1,"1FK70225AK211DG2"]
["1FK7022-5AK21-1DG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2111,"ΤΕΜ",1,"MC",1,"1FK70225AK211DG3"]
["1FK7022-5AK21-1DG5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2223,"ΤΕΜ",1,"MC",1,"1FK70225AK211DG5"]
["1FK7022-5AK21-1DG8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2344,"ΤΕΜ",1,"MC",1,"1FK70225AK211DG8"]
["1FK7022-5AK21-1DH0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2317,"ΤΕΜ",1,"MC",1,"1FK70225AK211DH0"]
["1FK7022-5AK21-1DH2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2430,"ΤΕΜ",1,"MC",1,"1FK70225AK211DH2"]
["1FK7022-5AK21-1DH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2371,"ΤΕΜ",1,"MC",1,"1FK70225AK211DH3"]
["1FK7022-5AK21-1DH5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2484,"ΤΕΜ",1,"MC",1,"1FK70225AK211DH5"]
["1FK7022-5AK21-1DH8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2605,"ΤΕΜ",1,"MC",1,"1FK70225AK211DH8"]
["1FK7022-5AK21-1LA0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2605,"ΤΕΜ",1,"MC",1,"1FK70225AK211LA0"]
["1FK7022-5AK21-1LA2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2717,"ΤΕΜ",1,"MC",1,"1FK70225AK211LA2"]
["1FK7022-5AK21-1LA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2659,"ΤΕΜ",1,"MC",1,"1FK70225AK211LA3"]
["1FK7022-5AK21-1LA5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2772,"ΤΕΜ",1,"MC",1,"1FK70225AK211LA5"]
["1FK7022-5AK21-1LA8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2893,"ΤΕΜ",1,"MC",1,"1FK70225AK211LA8"]
["1FK7022-5AK21-1LB0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2869,"ΤΕΜ",1,"MC",1,"1FK70225AK211LB0"]
["1FK7022-5AK21-1LB2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2981,"ΤΕΜ",1,"MC",1,"1FK70225AK211LB2"]
["1FK7022-5AK21-1LB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2923,"ΤΕΜ",1,"MC",1,"1FK70225AK211LB3"]
["1FK7022-5AK21-1LB5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3036,"ΤΕΜ",1,"MC",1,"1FK70225AK211LB5"]
["1FK7022-5AK21-1LB8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3156,"ΤΕΜ",1,"MC",1,"1FK70225AK211LB8"]
["1FK7022-5AK21-1LG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2501,"ΤΕΜ",1,"MC",1,"1FK70225AK211LG0"]
["1FK7022-5AK21-1LG2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2614,"ΤΕΜ",1,"MC",1,"1FK70225AK211LG2"]
["1FK7022-5AK21-1LG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2555,"ΤΕΜ",1,"MC",1,"1FK70225AK211LG3"]
["1FK7022-5AK21-1LG5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2668,"ΤΕΜ",1,"MC",1,"1FK70225AK211LG5"]
["1FK7022-5AK21-1LG8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2789,"ΤΕΜ",1,"MC",1,"1FK70225AK211LG8"]
["1FK7022-5AK21-1LH0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2762,"ΤΕΜ",1,"MC",1,"1FK70225AK211LH0"]
["1FK7022-5AK21-1LH2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2874,"ΤΕΜ",1,"MC",1,"1FK70225AK211LH2"]
["1FK7022-5AK21-1LH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2816,"ΤΕΜ",1,"MC",1,"1FK70225AK211LH3"]
["1FK7022-5AK21-1LH5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2929,"ΤΕΜ",1,"MC",1,"1FK70225AK211LH5"]
["1FK7022-5AK21-1LH8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3049,"ΤΕΜ",1,"MC",1,"1FK70225AK211LH8"]
["1FK7022-5AK21-1PA0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1454,"ΤΕΜ",1,"MC",1,"1FK70225AK211PA0"]
["1FK7022-5AK21-1PA2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1566,"ΤΕΜ",1,"MC",1,"1FK70225AK211PA2"]
["1FK7022-5AK21-1PA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1508,"ΤΕΜ",1,"MC",1,"1FK70225AK211PA3"]
["1FK7022-5AK21-1PA5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1621,"ΤΕΜ",1,"MC",1,"1FK70225AK211PA5"]
["1FK7022-5AK21-1PA8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1741,"ΤΕΜ",1,"MC",1,"1FK70225AK211PA8"]
["1FK7022-5AK21-1PB0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1718,"ΤΕΜ",1,"MC",1,"1FK70225AK211PB0"]
["1FK7022-5AK21-1PB2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1830,"ΤΕΜ",1,"MC",1,"1FK70225AK211PB2"]
["1FK7022-5AK21-1PB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1772,"ΤΕΜ",1,"MC",1,"1FK70225AK211PB3"]
["1FK7022-5AK21-1PB5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1885,"ΤΕΜ",1,"MC",1,"1FK70225AK211PB5"]
["1FK7022-5AK21-1PB8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2005,"ΤΕΜ",1,"MC",1,"1FK70225AK211PB8"]
["1FK7022-5AK21-1PG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1350,"ΤΕΜ",1,"MC",1,"1FK70225AK211PG0"]
["1FK7022-5AK21-1PG2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1463,"ΤΕΜ",1,"MC",1,"1FK70225AK211PG2"]
["1FK7022-5AK21-1PG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1404,"ΤΕΜ",1,"MC",1,"1FK70225AK211PG3"]
["1FK7022-5AK21-1PG5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1517,"ΤΕΜ",1,"MC",1,"1FK70225AK211PG5"]
["1FK7022-5AK21-1PG8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1638,"ΤΕΜ",1,"MC",1,"1FK70225AK211PG8"]
["1FK7022-5AK21-1PH0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1611,"ΤΕΜ",1,"MC",1,"1FK70225AK211PH0"]
["1FK7022-5AK21-1PH2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1723,"ΤΕΜ",1,"MC",1,"1FK70225AK211PH2"]
["1FK7022-5AK21-1PH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1665,"ΤΕΜ",1,"MC",1,"1FK70225AK211PH3"]
["1FK7022-5AK21-1PH5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1778,"ΤΕΜ",1,"MC",1,"1FK70225AK211PH5"]
["1FK7022-5AK21-1PH8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1898,"ΤΕΜ",1,"MC",1,"1FK70225AK211PH8"]
["1FK7022-5AK21-1UA0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1419,"ΤΕΜ",1,"MC",1,"1FK70225AK211UA0"]
["1FK7022-5AK21-1UA2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1532,"ΤΕΜ",1,"MC",1,"1FK70225AK211UA2"]
["1FK7022-5AK21-1UA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1474,"ΤΕΜ",1,"MC",1,"1FK70225AK211UA3"]
["1FK7022-5AK21-1UA5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1586,"ΤΕΜ",1,"MC",1,"1FK70225AK211UA5"]
["1FK7022-5AK21-1UA8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1707,"ΤΕΜ",1,"MC",1,"1FK70225AK211UA8"]
["1FK7022-5AK21-1UB0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1683,"ΤΕΜ",1,"MC",1,"1FK70225AK211UB0"]
["1FK7022-5AK21-1UB2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1796,"ΤΕΜ",1,"MC",1,"1FK70225AK211UB2"]
["1FK7022-5AK21-1UB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1738,"ΤΕΜ",1,"MC",1,"1FK70225AK211UB3"]
["1FK7022-5AK21-1UB5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1850,"ΤΕΜ",1,"MC",1,"1FK70225AK211UB5"]
["1FK7022-5AK21-1UB8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1971,"ΤΕΜ",1,"MC",1,"1FK70225AK211UB8"]
["1FK7022-5AK21-1UG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1315,"ΤΕΜ",1,"MC",1,"1FK70225AK211UG0"]
["1FK7022-5AK21-1UG2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1428,"ΤΕΜ",1,"MC",1,"1FK70225AK211UG2"]
["1FK7022-5AK21-1UG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1370,"ΤΕΜ",1,"MC",1,"1FK70225AK211UG3"]
["1FK7022-5AK21-1UG5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1483,"ΤΕΜ",1,"MC",1,"1FK70225AK211UG5"]
["1FK7022-5AK21-1UG8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1603,"ΤΕΜ",1,"MC",1,"1FK70225AK211UG8"]
["1FK7022-5AK21-1UH0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1576,"ΤΕΜ",1,"MC",1,"1FK70225AK211UH0"]
["1FK7022-5AK21-1UH2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1689,"ΤΕΜ",1,"MC",1,"1FK70225AK211UH2"]
["1FK7022-5AK21-1UH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1631,"ΤΕΜ",1,"MC",1,"1FK70225AK211UH3"]
["1FK7022-5AK21-1UH5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1743,"ΤΕΜ",1,"MC",1,"1FK70225AK211UH5"]
["1FK7022-5AK21-1UH8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1864,"ΤΕΜ",1,"MC",1,"1FK70225AK211UH8"]
["1FK7022-5AK21-1VA0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1981,"ΤΕΜ",1,"MC",1,"1FK70225AK211VA0"]
["1FK7022-5AK21-1VA2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2094,"ΤΕΜ",1,"MC",1,"1FK70225AK211VA2"]
["1FK7022-5AK21-1VA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2036,"ΤΕΜ",1,"MC",1,"1FK70225AK211VA3"]
["1FK7022-5AK21-1VA5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2149,"ΤΕΜ",1,"MC",1,"1FK70225AK211VA5"]
["1FK7022-5AK21-1VA8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2269,"ΤΕΜ",1,"MC",1,"1FK70225AK211VA8"]
["1FK7022-5AK21-1VB0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2245,"ΤΕΜ",1,"MC",1,"1FK70225AK211VB0"]
["1FK7022-5AK21-1VB2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2358,"ΤΕΜ",1,"MC",1,"1FK70225AK211VB2"]
["1FK7022-5AK21-1VB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2300,"ΤΕΜ",1,"MC",1,"1FK70225AK211VB3"]
["1FK7022-5AK21-1VB5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2412,"ΤΕΜ",1,"MC",1,"1FK70225AK211VB5"]
["1FK7022-5AK21-1VB8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2533,"ΤΕΜ",1,"MC",1,"1FK70225AK211VB8"]
["1FK7022-5AK21-1VG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1877,"ΤΕΜ",1,"MC",1,"1FK70225AK211VG0"]
["1FK7022-5AK21-1VG2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1990,"ΤΕΜ",1,"MC",1,"1FK70225AK211VG2"]
["1FK7022-5AK21-1VG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1932,"ΤΕΜ",1,"MC",1,"1FK70225AK211VG3"]
["1FK7022-5AK21-1VG5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2045,"ΤΕΜ",1,"MC",1,"1FK70225AK211VG5"]
["1FK7022-5AK21-1VG8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2165,"ΤΕΜ",1,"MC",1,"1FK70225AK211VG8"]
["1FK7022-5AK21-1VH0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2138,"ΤΕΜ",1,"MC",1,"1FK70225AK211VH0"]
["1FK7022-5AK21-1VH2","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2251,"ΤΕΜ",1,"MC",1,"1FK70225AK211VH2"]
["1FK7022-5AK21-1VH3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2193,"ΤΕΜ",1,"MC",1,"1FK70225AK211VH3"]
["1FK7022-5AK21-1VH5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2306,"ΤΕΜ",1,"MC",1,"1FK70225AK211VH5"]
["1FK7022-5AK21-1VH8","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2426,"ΤΕΜ",1,"MC",1,"1FK70225AK211VH8"]
["1FK7022-5AK24-1AA3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1905,"ΤΕΜ",1,"MC",1,"1FK70225AK241AA3"]
["1FK7022-5AK24-1AA5","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2017,"ΤΕΜ",1,"MC",1,"1FK70225AK241AA5"]
["1FK7022-5AK24-1AB0","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2114,"ΤΕΜ",1,"MC",1,"1FK70225AK241AB0"]
["1FK7022-5AK24-1JG3","SIMOTICS S Synchronous servo motor 1FK7 Compact, DC link 300V 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1643,"ΤΕΜ",1,"MC",1,"1FK70225AK241JG3"]
["1FK7022-5AK71-1DA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2160,"ΤΕΜ",1,"MC",1,"1FK70225AK711DA0"]
["1FK7022-5AK71-1DA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2273,"ΤΕΜ",1,"MC",1,"1FK70225AK711DA2"]
["1FK7022-5AK71-1DA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2214,"ΤΕΜ",1,"MC",1,"1FK70225AK711DA3"]
["1FK7022-5AK71-1DA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2327,"ΤΕΜ",1,"MC",1,"1FK70225AK711DA5"]
["1FK7022-5AK71-1DA8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2448,"ΤΕΜ",1,"MC",1,"1FK70225AK711DA8"]
["1FK7022-5AK71-1DB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2424,"ΤΕΜ",1,"MC",1,"1FK70225AK711DB0"]
["1FK7022-5AK71-1DB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2536,"ΤΕΜ",1,"MC",1,"1FK70225AK711DB2"]
["1FK7022-5AK71-1DB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2478,"ΤΕΜ",1,"MC",1,"1FK70225AK711DB3"]
["1FK7022-5AK71-1DB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2591,"ΤΕΜ",1,"MC",1,"1FK70225AK711DB5"]
["1FK7022-5AK71-1DB8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2711,"ΤΕΜ",1,"MC",1,"1FK70225AK711DB8"]
["1FK7022-5AK71-1DG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2056,"ΤΕΜ",1,"MC",1,"1FK70225AK711DG0"]
["1FK7022-5AK71-1DG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2169,"ΤΕΜ",1,"MC",1,"1FK70225AK711DG2"]
["1FK7022-5AK71-1DG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2111,"ΤΕΜ",1,"MC",1,"1FK70225AK711DG3"]
["1FK7022-5AK71-1DG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2223,"ΤΕΜ",1,"MC",1,"1FK70225AK711DG5"]
["1FK7022-5AK71-1DG8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2344,"ΤΕΜ",1,"MC",1,"1FK70225AK711DG8"]
["1FK7022-5AK71-1DH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2317,"ΤΕΜ",1,"MC",1,"1FK70225AK711DH0"]
["1FK7022-5AK71-1DH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2430,"ΤΕΜ",1,"MC",1,"1FK70225AK711DH2"]
["1FK7022-5AK71-1DH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2371,"ΤΕΜ",1,"MC",1,"1FK70225AK711DH3"]
["1FK7022-5AK71-1DH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2484,"ΤΕΜ",1,"MC",1,"1FK70225AK711DH5"]
["1FK7022-5AK71-1DH8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2605,"ΤΕΜ",1,"MC",1,"1FK70225AK711DH8"]
["1FK7022-5AK71-1LA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2605,"ΤΕΜ",1,"MC",1,"1FK70225AK711LA0"]
["1FK7022-5AK71-1LA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2717,"ΤΕΜ",1,"MC",1,"1FK70225AK711LA2"]
["1FK7022-5AK71-1LA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2659,"ΤΕΜ",1,"MC",1,"1FK70225AK711LA3"]
["1FK7022-5AK71-1LA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2772,"ΤΕΜ",1,"MC",1,"1FK70225AK711LA5"]
["1FK7022-5AK71-1LA8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2893,"ΤΕΜ",1,"MC",1,"1FK70225AK711LA8"]
["1FK7022-5AK71-1LB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2869,"ΤΕΜ",1,"MC",1,"1FK70225AK711LB0"]
["1FK7022-5AK71-1LB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2981,"ΤΕΜ",1,"MC",1,"1FK70225AK711LB2"]
["1FK7022-5AK71-1LB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2923,"ΤΕΜ",1,"MC",1,"1FK70225AK711LB3"]
["1FK7022-5AK71-1LB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3036,"ΤΕΜ",1,"MC",1,"1FK70225AK711LB5"]
["1FK7022-5AK71-1LB8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3156,"ΤΕΜ",1,"MC",1,"1FK70225AK711LB8"]
["1FK7022-5AK71-1LG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2501,"ΤΕΜ",1,"MC",1,"1FK70225AK711LG0"]
["1FK7022-5AK71-1LG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2614,"ΤΕΜ",1,"MC",1,"1FK70225AK711LG2"]
["1FK7022-5AK71-1LG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2555,"ΤΕΜ",1,"MC",1,"1FK70225AK711LG3"]
["1FK7022-5AK71-1LG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2668,"ΤΕΜ",1,"MC",1,"1FK70225AK711LG5"]
["1FK7022-5AK71-1LG8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2789,"ΤΕΜ",1,"MC",1,"1FK70225AK711LG8"]
["1FK7022-5AK71-1LH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2762,"ΤΕΜ",1,"MC",1,"1FK70225AK711LH0"]
["1FK7022-5AK71-1LH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2874,"ΤΕΜ",1,"MC",1,"1FK70225AK711LH2"]
["1FK7022-5AK71-1LH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2816,"ΤΕΜ",1,"MC",1,"1FK70225AK711LH3"]
["1FK7022-5AK71-1LH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2929,"ΤΕΜ",1,"MC",1,"1FK70225AK711LH5"]
["1FK7022-5AK71-1LH8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 Absolute encoder 20BIT +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQ) Derating 10% due to absolute encoder PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3049,"ΤΕΜ",1,"MC",1,"1FK70225AK711LH8"]
["1FK7022-5AK71-1PA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1454,"ΤΕΜ",1,"MC",1,"1FK70225AK711PA0"]
["1FK7022-5AK71-1PA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1566,"ΤΕΜ",1,"MC",1,"1FK70225AK711PA2"]
["1FK7022-5AK71-1PA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1508,"ΤΕΜ",1,"MC",1,"1FK70225AK711PA3"]
["1FK7022-5AK71-1PA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1621,"ΤΕΜ",1,"MC",1,"1FK70225AK711PA5"]
["1FK7022-5AK71-1PA8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1741,"ΤΕΜ",1,"MC",1,"1FK70225AK711PA8"]
["1FK7022-5AK71-1PB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1718,"ΤΕΜ",1,"MC",1,"1FK70225AK711PB0"]
["1FK7022-5AK71-1PB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1830,"ΤΕΜ",1,"MC",1,"1FK70225AK711PB2"]
["1FK7022-5AK71-1PB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1772,"ΤΕΜ",1,"MC",1,"1FK70225AK711PB3"]
["1FK7022-5AK71-1PB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1885,"ΤΕΜ",1,"MC",1,"1FK70225AK711PB5"]
["1FK7022-5AK71-1PB8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2005,"ΤΕΜ",1,"MC",1,"1FK70225AK711PB8"]
["1FK7022-5AK71-1PG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1350,"ΤΕΜ",1,"MC",1,"1FK70225AK711PG0"]
["1FK7022-5AK71-1PG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1463,"ΤΕΜ",1,"MC",1,"1FK70225AK711PG2"]
["1FK7022-5AK71-1PG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1404,"ΤΕΜ",1,"MC",1,"1FK70225AK711PG3"]
["1FK7022-5AK71-1PG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1517,"ΤΕΜ",1,"MC",1,"1FK70225AK711PG5"]
["1FK7022-5AK71-1PG8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1638,"ΤΕΜ",1,"MC",1,"1FK70225AK711PG8"]
["1FK7022-5AK71-1PH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1611,"ΤΕΜ",1,"MC",1,"1FK70225AK711PH0"]
["1FK7022-5AK71-1PH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1723,"ΤΕΜ",1,"MC",1,"1FK70225AK711PH2"]
["1FK7022-5AK71-1PH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1665,"ΤΕΜ",1,"MC",1,"1FK70225AK711PH3"]
["1FK7022-5AK71-1PH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1778,"ΤΕΜ",1,"MC",1,"1FK70225AK711PH5"]
["1FK7022-5AK71-1PH8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1898,"ΤΕΜ",1,"MC",1,"1FK70225AK711PH8"]
["1FK7022-5AK71-1UA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1454,"ΤΕΜ",1,"MC",1,"1FK70225AK711UA0"]
["1FK7022-5AK71-1UA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1566,"ΤΕΜ",1,"MC",1,"1FK70225AK711UA2"]
["1FK7022-5AK71-1UA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1508,"ΤΕΜ",1,"MC",1,"1FK70225AK711UA3"]
["1FK7022-5AK71-1UA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1621,"ΤΕΜ",1,"MC",1,"1FK70225AK711UA5"]
["1FK7022-5AK71-1UA8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1741,"ΤΕΜ",1,"MC",1,"1FK70225AK711UA8"]
["1FK7022-5AK71-1UB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1718,"ΤΕΜ",1,"MC",1,"1FK70225AK711UB0"]
["1FK7022-5AK71-1UB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1830,"ΤΕΜ",1,"MC",1,"1FK70225AK711UB2"]
["1FK7022-5AK71-1UB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1772,"ΤΕΜ",1,"MC",1,"1FK70225AK711UB3"]
["1FK7022-5AK71-1UB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1885,"ΤΕΜ",1,"MC",1,"1FK70225AK711UB5"]
["1FK7022-5AK71-1UB8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2005,"ΤΕΜ",1,"MC",1,"1FK70225AK711UB8"]
["1FK7022-5AK71-1UG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1350,"ΤΕΜ",1,"MC",1,"1FK70225AK711UG0"]
["1FK7022-5AK71-1UG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1463,"ΤΕΜ",1,"MC",1,"1FK70225AK711UG2"]
["1FK7022-5AK71-1UG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1404,"ΤΕΜ",1,"MC",1,"1FK70225AK711UG3"]
["1FK7022-5AK71-1UG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1517,"ΤΕΜ",1,"MC",1,"1FK70225AK711UG5"]
["1FK7022-5AK71-1UG8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1638,"ΤΕΜ",1,"MC",1,"1FK70225AK711UG8"]
["1FK7022-5AK71-1UH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1611,"ΤΕΜ",1,"MC",1,"1FK70225AK711UH0"]
["1FK7022-5AK71-1UH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1723,"ΤΕΜ",1,"MC",1,"1FK70225AK711UH2"]
["1FK7022-5AK71-1UH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1665,"ΤΕΜ",1,"MC",1,"1FK70225AK711UH3"]
["1FK7022-5AK71-1UH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1778,"ΤΕΜ",1,"MC",1,"1FK70225AK711UH5"]
["1FK7022-5AK71-1UH8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1898,"ΤΕΜ",1,"MC",1,"1FK70225AK711UH8"]
["1FK7022-5AK71-1VA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1981,"ΤΕΜ",1,"MC",1,"1FK70225AK711VA0"]
["1FK7022-5AK71-1VA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2094,"ΤΕΜ",1,"MC",1,"1FK70225AK711VA2"]
["1FK7022-5AK71-1VA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2036,"ΤΕΜ",1,"MC",1,"1FK70225AK711VA3"]
["1FK7022-5AK71-1VA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2149,"ΤΕΜ",1,"MC",1,"1FK70225AK711VA5"]
["1FK7022-5AK71-1VA8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2269,"ΤΕΜ",1,"MC",1,"1FK70225AK711VA8"]
["1FK7022-5AK71-1VB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2245,"ΤΕΜ",1,"MC",1,"1FK70225AK711VB0"]
["1FK7022-5AK71-1VB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2358,"ΤΕΜ",1,"MC",1,"1FK70225AK711VB2"]
["1FK7022-5AK71-1VB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2300,"ΤΕΜ",1,"MC",1,"1FK70225AK711VB3"]
["1FK7022-5AK71-1VB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2412,"ΤΕΜ",1,"MC",1,"1FK70225AK711VB5"]
["1FK7022-5AK71-1VB8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2533,"ΤΕΜ",1,"MC",1,"1FK70225AK711VB8"]
["1FK7022-5AK71-1VG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1877,"ΤΕΜ",1,"MC",1,"1FK70225AK711VG0"]
["1FK7022-5AK71-1VG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1990,"ΤΕΜ",1,"MC",1,"1FK70225AK711VG2"]
["1FK7022-5AK71-1VG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1932,"ΤΕΜ",1,"MC",1,"1FK70225AK711VG3"]
["1FK7022-5AK71-1VG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2045,"ΤΕΜ",1,"MC",1,"1FK70225AK711VG5"]
["1FK7022-5AK71-1VG8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2165,"ΤΕΜ",1,"MC",1,"1FK70225AK711VG8"]
["1FK7022-5AK71-1VH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2138,"ΤΕΜ",1,"MC",1,"1FK70225AK711VH0"]
["1FK7022-5AK71-1VH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2251,"ΤΕΜ",1,"MC",1,"1FK70225AK711VH2"]
["1FK7022-5AK71-1VH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2193,"ΤΕΜ",1,"MC",1,"1FK70225AK711VH3"]
["1FK7022-5AK71-1VH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2306,"ΤΕΜ",1,"MC",1,"1FK70225AK711VH5"]
["1FK7022-5AK71-1VH8","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2426,"ΤΕΜ",1,"MC",1,"1FK70225AK711VH8"]
["1FK7022-5AK74-1AA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1850,"ΤΕΜ",1,"MC",1,"1FK70225AK741AA0"]
["1FK7022-5AK74-1AA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1963,"ΤΕΜ",1,"MC",1,"1FK70225AK741AA2"]
["1FK7022-5AK74-1AA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1905,"ΤΕΜ",1,"MC",1,"1FK70225AK741AA3"]
["1FK7022-5AK74-1AA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2017,"ΤΕΜ",1,"MC",1,"1FK70225AK741AA5"]
["1FK7022-5AK74-1AB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2114,"ΤΕΜ",1,"MC",1,"1FK70225AK741AB0"]
["1FK7022-5AK74-1AB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2227,"ΤΕΜ",1,"MC",1,"1FK70225AK741AB2"]
["1FK7022-5AK74-1AB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2168,"ΤΕΜ",1,"MC",1,"1FK70225AK741AB3"]
["1FK7022-5AK74-1AB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2281,"ΤΕΜ",1,"MC",1,"1FK70225AK741AB5"]
["1FK7022-5AK74-1AG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1746,"ΤΕΜ",1,"MC",1,"1FK70225AK741AG0"]
["1FK7022-5AK74-1AG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1859,"ΤΕΜ",1,"MC",1,"1FK70225AK741AG2"]
["1FK7022-5AK74-1AG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1801,"ΤΕΜ",1,"MC",1,"1FK70225AK741AG3"]
["1FK7022-5AK74-1AG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1913,"ΤΕΜ",1,"MC",1,"1FK70225AK741AG5"]
["1FK7022-5AK74-1AH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2007,"ΤΕΜ",1,"MC",1,"1FK70225AK741AH0"]
["1FK7022-5AK74-1AH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2120,"ΤΕΜ",1,"MC",1,"1FK70225AK741AH2"]
["1FK7022-5AK74-1AH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2062,"ΤΕΜ",1,"MC",1,"1FK70225AK741AH3"]
["1FK7022-5AK74-1AH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2174,"ΤΕΜ",1,"MC",1,"1FK70225AK741AH5"]
["1FK7022-5AK74-1HA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2317,"ΤΕΜ",1,"MC",1,"1FK70225AK741HA0"]
["1FK7022-5AK74-1HA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2430,"ΤΕΜ",1,"MC",1,"1FK70225AK741HA2"]
["1FK7022-5AK74-1HA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2372,"ΤΕΜ",1,"MC",1,"1FK70225AK741HA3"]
["1FK7022-5AK74-1HA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2484,"ΤΕΜ",1,"MC",1,"1FK70225AK741HA5"]
["1FK7022-5AK74-1HB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2581,"ΤΕΜ",1,"MC",1,"1FK70225AK741HB0"]
["1FK7022-5AK74-1HB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2694,"ΤΕΜ",1,"MC",1,"1FK70225AK741HB2"]
["1FK7022-5AK74-1HB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2635,"ΤΕΜ",1,"MC",1,"1FK70225AK741HB3"]
["1FK7022-5AK74-1HB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2748,"ΤΕΜ",1,"MC",1,"1FK70225AK741HB5"]
["1FK7022-5AK74-1HG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2213,"ΤΕΜ",1,"MC",1,"1FK70225AK741HG0"]
["1FK7022-5AK74-1HG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2326,"ΤΕΜ",1,"MC",1,"1FK70225AK741HG2"]
["1FK7022-5AK74-1HG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2268,"ΤΕΜ",1,"MC",1,"1FK70225AK741HG3"]
["1FK7022-5AK74-1HG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2380,"ΤΕΜ",1,"MC",1,"1FK70225AK741HG5"]
["1FK7022-5AK74-1HH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2474,"ΤΕΜ",1,"MC",1,"1FK70225AK741HH0"]
["1FK7022-5AK74-1HH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2587,"ΤΕΜ",1,"MC",1,"1FK70225AK741HH2"]
["1FK7022-5AK74-1HH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2529,"ΤΕΜ",1,"MC",1,"1FK70225AK741HH3"]
["1FK7022-5AK74-1HH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2641,"ΤΕΜ",1,"MC",1,"1FK70225AK741HH5"]
["1FK7022-5AK74-1JA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1693,"ΤΕΜ",1,"MC",1,"1FK70225AK741JA0"]
["1FK7022-5AK74-1JA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1805,"ΤΕΜ",1,"MC",1,"1FK70225AK741JA2"]
["1FK7022-5AK74-1JA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1747,"ΤΕΜ",1,"MC",1,"1FK70225AK741JA3"]
["1FK7022-5AK74-1JA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1860,"ΤΕΜ",1,"MC",1,"1FK70225AK741JA5"]
["1FK7022-5AK74-1JB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1956,"ΤΕΜ",1,"MC",1,"1FK70225AK741JB0"]
["1FK7022-5AK74-1JB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2069,"ΤΕΜ",1,"MC",1,"1FK70225AK741JB2"]
["1FK7022-5AK74-1JB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2011,"ΤΕΜ",1,"MC",1,"1FK70225AK741JB3"]
["1FK7022-5AK74-1JB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2124,"ΤΕΜ",1,"MC",1,"1FK70225AK741JB5"]
["1FK7022-5AK74-1JG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1589,"ΤΕΜ",1,"MC",1,"1FK70225AK741JG0"]
["1FK7022-5AK74-1JG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1701,"ΤΕΜ",1,"MC",1,"1FK70225AK741JG2"]
["1FK7022-5AK74-1JG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1643,"ΤΕΜ",1,"MC",1,"1FK70225AK741JG3"]
["1FK7022-5AK74-1JG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1756,"ΤΕΜ",1,"MC",1,"1FK70225AK741JG5"]
["1FK7022-5AK74-1JH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1850,"ΤΕΜ",1,"MC",1,"1FK70225AK741JH0"]
["1FK7022-5AK74-1JH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1962,"ΤΕΜ",1,"MC",1,"1FK70225AK741JH2"]
["1FK7022-5AK74-1JH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1904,"ΤΕΜ",1,"MC",1,"1FK70225AK741JH3"]
["1FK7022-5AK74-1JH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2017,"ΤΕΜ",1,"MC",1,"1FK70225AK741JH5"]
["1FK7022-5AK74-1SA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1163,"ΤΕΜ",1,"MC",1,"1FK70225AK741SA0"]
["1FK7022-5AK74-1SA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1276,"ΤΕΜ",1,"MC",1,"1FK70225AK741SA2"]
["1FK7022-5AK74-1SA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1218,"ΤΕΜ",1,"MC",1,"1FK70225AK741SA3"]
["1FK7022-5AK74-1SA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1331,"ΤΕΜ",1,"MC",1,"1FK70225AK741SA5"]
["1FK7022-5AK74-1SB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1427,"ΤΕΜ",1,"MC",1,"1FK70225AK741SB0"]
["1FK7022-5AK74-1SB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1540,"ΤΕΜ",1,"MC",1,"1FK70225AK741SB2"]
["1FK7022-5AK74-1SB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1482,"ΤΕΜ",1,"MC",1,"1FK70225AK741SB3"]
["1FK7022-5AK74-1SB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1594,"ΤΕΜ",1,"MC",1,"1FK70225AK741SB5"]
["1FK7022-5AK74-1SG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1059,"ΤΕΜ",1,"MC",1,"1FK70225AK741SG0"]
["1FK7022-5AK74-1SG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1172,"ΤΕΜ",1,"MC",1,"1FK70225AK741SG2"]
["1FK7022-5AK74-1SG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1114,"ΤΕΜ",1,"MC",1,"1FK70225AK741SG3"]
["1FK7022-5AK74-1SG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1227,"ΤΕΜ",1,"MC",1,"1FK70225AK741SG5"]
["1FK7022-5AK74-1SH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1320,"ΤΕΜ",1,"MC",1,"1FK70225AK741SH0"]
["1FK7022-5AK74-1SH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1433,"ΤΕΜ",1,"MC",1,"1FK70225AK741SH2"]
["1FK7022-5AK74-1SH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1375,"ΤΕΜ",1,"MC",1,"1FK70225AK741SH3"]
["1FK7022-5AK74-1SH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1488,"ΤΕΜ",1,"MC",1,"1FK70225AK741SH5"]
["1FK7022-5AK74-1TA0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1163,"ΤΕΜ",1,"MC",1,"1FK70225AK741TA0"]
["1FK7022-5AK74-1TA2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1276,"ΤΕΜ",1,"MC",1,"1FK70225AK741TA2"]
["1FK7022-5AK74-1TA3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1218,"ΤΕΜ",1,"MC",1,"1FK70225AK741TA3"]
["1FK7022-5AK74-1TA5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1331,"ΤΕΜ",1,"MC",1,"1FK70225AK741TA5"]
["1FK7022-5AK74-1TB0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1427,"ΤΕΜ",1,"MC",1,"1FK70225AK741TB0"]
["1FK7022-5AK74-1TB2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1540,"ΤΕΜ",1,"MC",1,"1FK70225AK741TB2"]
["1FK7022-5AK74-1TB3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1482,"ΤΕΜ",1,"MC",1,"1FK70225AK741TB3"]
["1FK7022-5AK74-1TB5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1594,"ΤΕΜ",1,"MC",1,"1FK70225AK741TB5"]
["1FK7022-5AK74-1TG0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1059,"ΤΕΜ",1,"MC",1,"1FK70225AK741TG0"]
["1FK7022-5AK74-1TG2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1172,"ΤΕΜ",1,"MC",1,"1FK70225AK741TG2"]
["1FK7022-5AK74-1TG3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1114,"ΤΕΜ",1,"MC",1,"1FK70225AK741TG3"]
["1FK7022-5AK74-1TG5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1227,"ΤΕΜ",1,"MC",1,"1FK70225AK741TG5"]
["1FK7022-5AK74-1TH0","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1320,"ΤΕΜ",1,"MC",1,"1FK70225AK741TH0"]
["1FK7022-5AK74-1TH2","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1433,"ΤΕΜ",1,"MC",1,"1FK70225AK741TH2"]
["1FK7022-5AK74-1TH3","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1375,"ΤΕΜ",1,"MC",1,"1FK70225AK741TH3"]
["1FK7022-5AK74-1TH5","SIMOTICS S Synchronous servo motor 1FK7 Compact 0.85Nm, 100K, 6000rpm 0.38kW, Naturally cooled Power/signal connectors Connector can be rotated by 270Β° IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1488,"ΤΕΜ",1,"MC",1,"1FK70225AK741TH5"]
["1FK7022-5AK74-8HG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, 0.85Nm 100K, 6000rpm, 0.38kW Naturally cooled Bare cable end 0.5m Outlet directions DE with connector size 1 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2463,"ΤΕΜ",1,"MC",1,"1FK70225AK748HG0"]
["1FK7022-5AK74-8HH2","SIMOTICS S Synchronous servo motor 1FK7 Compact, 0.85Nm 100K, 6000rpm, 0.38kW Naturally cooled Bare cable end 0.5m Outlet directions DE with connector size 1 IMB 5 design (IM V1, IM V3) Flange 1, with Pt1000 temperature sensor ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2836,"ΤΕΜ",1,"MC",1,"1FK70225AK748HH2"]
["1FK7024-5AK71-1LB3","SIMOTICS S Synchronous servo motor 1FK7 Compact, 1.1Nm 100K, 6000rpm, 0.50kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° absolute encoder 512 S/R (encoder A-512) with DRIVE-CLiQ interface Derating 10% due to absolute encoder Shaft with feather key tolerance N with holding brake Degree of protection IP64 paint finish RAL7016",3103,"ΤΕΜ",1,"MC",1,"1FK70245AK711LB3"]
["1FK7024-5AK71-1LG0","SIMOTICS S Synchronous servo motor 1FK7 Compact, 1.1Nm 100K, 6000rpm, 0.50kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° absolute encoder 512 S/R (encoder A-512) with DRIVE-CLiQ interface Derating 10% due to absolute encoder Smooth shaft Tolerance N without holding brake Degree of protection IP65",2681,"ΤΕΜ",1,"MC",1,"1FK70245AK711LG0"]
["1FK7024-5AK71-1LG2","SIMOTICS S Synchronous servo motor 1FK7 Compact, 1.1Nm 100K, 6000rpm, 0.50kW Naturally cooled IM B5 (IM V1, IM V3) power/signal connectors Connector can be rotated by 270Β° absolute encoder 512 S/R (encoder A-512) with DRIVE-CLiQ interface Derating 10% due to absolute encoder Smooth shaft Tolerance N without holding brake Degree of protection IP65 DE flange IP67",2793,"ΤΕΜ",1,"MC",1,"1FK70245AK711LG2"]
["1FK7032-2AF21-1BA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",2104,"ΤΕΜ",1,"MC",1,"1FK70322AF211BA0"]
["1FK7032-2AF21-1BA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",2212,"ΤΕΜ",1,"MC",1,"1FK70322AF211BA1"]
["1FK7032-2AF21-1BA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",2212,"ΤΕΜ",1,"MC",1,"1FK70322AF211BA2"]
["1FK7032-2AF21-1BB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",2356,"ΤΕΜ",1,"MC",1,"1FK70322AF211BB0"]
["1FK7032-2AF21-1BB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",2463,"ΤΕΜ",1,"MC",1,"1FK70322AF211BB1"]
["1FK7032-2AF21-1BB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",2463,"ΤΕΜ",1,"MC",1,"1FK70322AF211BB2"]
["1FK7032-2AF21-1BG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",2005,"ΤΕΜ",1,"MC",1,"1FK70322AF211BG0"]
["1FK7032-2AF21-1BG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",2113,"ΤΕΜ",1,"MC",1,"1FK70322AF211BG1"]
["1FK7032-2AF21-1BG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",2113,"ΤΕΜ",1,"MC",1,"1FK70322AF211BG2"]
["1FK7032-2AF21-1BH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",2254,"ΤΕΜ",1,"MC",1,"1FK70322AF211BH0"]
["1FK7032-2AF21-1BH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",2361,"ΤΕΜ",1,"MC",1,"1FK70322AF211BH1"]
["1FK7032-2AF21-1BH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65, DE flange IP67",2361,"ΤΕΜ",1,"MC",1,"1FK70322AF211BH2"]
["1FK7032-2AF21-1CA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",2528,"ΤΕΜ",1,"MC",1,"1FK70322AF211CA0"]
["1FK7032-2AF21-1CA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",2635,"ΤΕΜ",1,"MC",1,"1FK70322AF211CA1"]
["1FK7032-2AF21-1CA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",2635,"ΤΕΜ",1,"MC",1,"1FK70322AF211CA2"]
["1FK7032-2AF21-1CB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",2779,"ΤΕΜ",1,"MC",1,"1FK70322AF211CB0"]
["1FK7032-2AF21-1CB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",2887,"ΤΕΜ",1,"MC",1,"1FK70322AF211CB1"]
["1FK7032-2AF21-1CB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",2887,"ΤΕΜ",1,"MC",1,"1FK70322AF211CB2"]
["1FK7032-2AF21-1CG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",2429,"ΤΕΜ",1,"MC",1,"1FK70322AF211CG0"]
["1FK7032-2AF21-1CG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",2537,"ΤΕΜ",1,"MC",1,"1FK70322AF211CG1"]
["1FK7032-2AF21-1CG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",2537,"ΤΕΜ",1,"MC",1,"1FK70322AF211CG2"]
["1FK7032-2AF21-1CH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",2678,"ΤΕΜ",1,"MC",1,"1FK70322AF211CH0"]
["1FK7032-2AF21-1CH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",2785,"ΤΕΜ",1,"MC",1,"1FK70322AF211CH1"]
["1FK7032-2AF21-1CH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65, DE flange IP67",2785,"ΤΕΜ",1,"MC",1,"1FK70322AF211CH2"]
["1FK7032-2AF21-1DA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2196,"ΤΕΜ",1,"MC",1,"1FK70322AF211DA0"]
["1FK7032-2AF21-1DA1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2302,"ΤΕΜ",1,"MC",1,"1FK70322AF211DA1"]
["1FK7032-2AF21-1DB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2448,"ΤΕΜ",1,"MC",1,"1FK70322AF211DB0"]
["1FK7032-2AF21-1DG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2097,"ΤΕΜ",1,"MC",1,"1FK70322AF211DG0"]
["1FK7032-2AF21-1DH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2346,"ΤΕΜ",1,"MC",1,"1FK70322AF211DH0"]
["1FK7032-2AF21-1FA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2620,"ΤΕΜ",1,"MC",1,"1FK70322AF211FA0"]
["1FK7032-2AF21-1FB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2871,"ΤΕΜ",1,"MC",1,"1FK70322AF211FB0"]
["1FK7032-2AF21-1FB1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2977,"ΤΕΜ",1,"MC",1,"1FK70322AF211FB1"]
["1FK7032-2AF21-1FG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2521,"ΤΕΜ",1,"MC",1,"1FK70322AF211FG0"]
["1FK7032-2AF21-1FH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2770,"ΤΕΜ",1,"MC",1,"1FK70322AF211FH0"]
["1FK7032-2AF21-1FH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2875,"ΤΕΜ",1,"MC",1,"1FK70322AF211FH2"]
["1FK7032-2AF21-1PA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP64",1432,"ΤΕΜ",1,"MC",1,"1FK70322AF211PA0"]
["1FK7032-2AF21-1PA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP65",1539,"ΤΕΜ",1,"MC",1,"1FK70322AF211PA1"]
["1FK7032-2AF21-1PA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1539,"ΤΕΜ",1,"MC",1,"1FK70322AF211PA2"]
["1FK7032-2AF21-1PB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP64",1683,"ΤΕΜ",1,"MC",1,"1FK70322AF211PB0"]
["1FK7032-2AF21-1PB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP65",1790,"ΤΕΜ",1,"MC",1,"1FK70322AF211PB1"]
["1FK7032-2AF21-1PB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1790,"ΤΕΜ",1,"MC",1,"1FK70322AF211PB2"]
["1FK7032-2AF21-1PG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP64",1333,"ΤΕΜ",1,"MC",1,"1FK70322AF211PG0"]
["1FK7032-2AF21-1PG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP65",1440,"ΤΕΜ",1,"MC",1,"1FK70322AF211PG1"]
["1FK7032-2AF21-1PG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1440,"ΤΕΜ",1,"MC",1,"1FK70322AF211PG2"]
["1FK7032-2AF21-1PH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP64",1581,"ΤΕΜ",1,"MC",1,"1FK70322AF211PH0"]
["1FK7032-2AF21-1PH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP65",1689,"ΤΕΜ",1,"MC",1,"1FK70322AF211PH1"]
["1FK7032-2AF21-1PH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1689,"ΤΕΜ",1,"MC",1,"1FK70322AF211PH2"]
["1FK7032-2AF21-1QA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",1550,"ΤΕΜ",1,"MC",1,"1FK70322AF211QA0"]
["1FK7032-2AF21-1QA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",1657,"ΤΕΜ",1,"MC",1,"1FK70322AF211QA1"]
["1FK7032-2AF21-1QA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1657,"ΤΕΜ",1,"MC",1,"1FK70322AF211QA2"]
["1FK7032-2AF21-1QB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",1801,"ΤΕΜ",1,"MC",1,"1FK70322AF211QB0"]
["1FK7032-2AF21-1QB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",1909,"ΤΕΜ",1,"MC",1,"1FK70322AF211QB1"]
["1FK7032-2AF21-1QB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",1909,"ΤΕΜ",1,"MC",1,"1FK70322AF211QB2"]
["1FK7032-2AF21-1QG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UZK=300V M0=1.2Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 power connector rotatable absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",1451,"ΤΕΜ",1,"MC",1,"1FK70322AF211QG0"]
["1FK7032-2AF21-1QG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",1558,"ΤΕΜ",1,"MC",1,"1FK70322AF211QG1"]
["1FK7032-2AF21-1QG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",1558,"ΤΕΜ",1,"MC",1,"1FK70322AF211QG2"]
["1FK7032-2AF21-1QH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",1700,"ΤΕΜ",1,"MC",1,"1FK70322AF211QH0"]
["1FK7032-2AF21-1QH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",1807,"ΤΕΜ",1,"MC",1,"1FK70322AF211QH1"]
["1FK7032-2AF21-1QH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65, DE flange IP67",1807,"ΤΕΜ",1,"MC",1,"1FK70322AF211QH2"]
["1FK7032-2AF21-1RA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",1979,"ΤΕΜ",1,"MC",1,"1FK70322AF211RA0"]
["1FK7032-2AF21-1RA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",2087,"ΤΕΜ",1,"MC",1,"1FK70322AF211RA1"]
["1FK7032-2AF21-1RA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",2087,"ΤΕΜ",1,"MC",1,"1FK70322AF211RA2"]
["1FK7032-2AF21-1RB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",2231,"ΤΕΜ",1,"MC",1,"1FK70322AF211RB0"]
["1FK7032-2AF21-1RB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",2338,"ΤΕΜ",1,"MC",1,"1FK70322AF211RB1"]
["1FK7032-2AF21-1RB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",2338,"ΤΕΜ",1,"MC",1,"1FK70322AF211RB2"]
["1FK7032-2AF21-1RG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",1880,"ΤΕΜ",1,"MC",1,"1FK70322AF211RG0"]
["1FK7032-2AF21-1RG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",1988,"ΤΕΜ",1,"MC",1,"1FK70322AF211RG1"]
["1FK7032-2AF21-1RG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",1988,"ΤΕΜ",1,"MC",1,"1FK70322AF211RG2"]
["1FK7032-2AF21-1RH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",2129,"ΤΕΜ",1,"MC",1,"1FK70322AF211RH0"]
["1FK7032-2AF21-1RH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",2236,"ΤΕΜ",1,"MC",1,"1FK70322AF211RH1"]
["1FK7032-2AF21-1RH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65, DE flange IP67",2236,"ΤΕΜ",1,"MC",1,"1FK70322AF211RH2"]
["1FK7032-2AF21-1UA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP64",1432,"ΤΕΜ",1,"MC",1,"1FK70322AF211UA0"]
["1FK7032-2AF21-1UA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP65",1539,"ΤΕΜ",1,"MC",1,"1FK70322AF211UA1"]
["1FK7032-2AF21-1UA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1539,"ΤΕΜ",1,"MC",1,"1FK70322AF211UA2"]
["1FK7032-2AF21-1UB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP64",1683,"ΤΕΜ",1,"MC",1,"1FK70322AF211UB0"]
["1FK7032-2AF21-1UB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP65",1790,"ΤΕΜ",1,"MC",1,"1FK70322AF211UB1"]
["1FK7032-2AF21-1UB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1790,"ΤΕΜ",1,"MC",1,"1FK70322AF211UB2"]
["1FK7032-2AF21-1UG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP64",1333,"ΤΕΜ",1,"MC",1,"1FK70322AF211UG0"]
["1FK7032-2AF21-1UG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP65",1440,"ΤΕΜ",1,"MC",1,"1FK70322AF211UG1"]
["1FK7032-2AF21-1UG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1440,"ΤΕΜ",1,"MC",1,"1FK70322AF211UG2"]
["1FK7032-2AF21-1UH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP64",1581,"ΤΕΜ",1,"MC",1,"1FK70322AF211UH0"]
["1FK7032-2AF21-1UH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP65",1689,"ΤΕΜ",1,"MC",1,"1FK70322AF211UH1"]
["1FK7032-2AF21-1UH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1689,"ΤΕΜ",1,"MC",1,"1FK70322AF211UH2"]
["1FK7032-2AF24-1EH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.31kW; UDC=300V; M0=1.2Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2509,"ΤΕΜ",1,"MC",1,"1FK70322AF241EH2"]
["1FK7032-2AF24-1SA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP64",1155,"ΤΕΜ",1,"MC",1,"1FK70322AF241SA0"]
["1FK7032-2AF24-1SA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP65",1263,"ΤΕΜ",1,"MC",1,"1FK70322AF241SA1"]
["1FK7032-2AF24-1SA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1263,"ΤΕΜ",1,"MC",1,"1FK70322AF241SA2"]
["1FK7032-2AF24-1SB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP64",1406,"ΤΕΜ",1,"MC",1,"1FK70322AF241SB0"]
["1FK7032-2AF24-1SB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP65",1514,"ΤΕΜ",1,"MC",1,"1FK70322AF241SB1"]
["1FK7032-2AF24-1SB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",1514,"ΤΕΜ",1,"MC",1,"1FK70322AF241SB2"]
["1FK7032-2AF24-1SG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP64",1056,"ΤΕΜ",1,"MC",1,"1FK70322AF241SG0"]
["1FK7032-2AF24-1SG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP65",1164,"ΤΕΜ",1,"MC",1,"1FK70322AF241SG1"]
["1FK7032-2AF24-1SG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP65 DE flange IP67",1164,"ΤΕΜ",1,"MC",1,"1FK70322AF241SG2"]
["1FK7032-2AF24-1SH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, type of protection IP64",1305,"ΤΕΜ",1,"MC",1,"1FK70322AF241SH0"]
["1FK7032-2AF24-1SH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, type of protection IP65",1412,"ΤΕΜ",1,"MC",1,"1FK70322AF241SH1"]
["1FK7032-2AF24-1SH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, degree of protection IP65 DE Flange IP67",1412,"ΤΕΜ",1,"MC",1,"1FK70322AF241SH2"]
["1FK7032-2AF24-1TA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP64",1155,"ΤΕΜ",1,"MC",1,"1FK70322AF241TA0"]
["1FK7032-2AF24-1TA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP65",1263,"ΤΕΜ",1,"MC",1,"1FK70322AF241TA1"]
["1FK7032-2AF24-1TA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1263,"ΤΕΜ",1,"MC",1,"1FK70322AF241TA2"]
["1FK7032-2AF24-1TB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP64",1406,"ΤΕΜ",1,"MC",1,"1FK70322AF241TB0"]
["1FK7032-2AF24-1TB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP65",1514,"ΤΕΜ",1,"MC",1,"1FK70322AF241TB1"]
["1FK7032-2AF24-1TB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",1514,"ΤΕΜ",1,"MC",1,"1FK70322AF241TB2"]
["1FK7032-2AF24-1TG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP64",1056,"ΤΕΜ",1,"MC",1,"1FK70322AF241TG0"]
["1FK7032-2AF24-1TG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP65",1164,"ΤΕΜ",1,"MC",1,"1FK70322AF241TG1"]
["1FK7032-2AF24-1TG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP65 DE flange IP67",1164,"ΤΕΜ",1,"MC",1,"1FK70322AF241TG2"]
["1FK7032-2AF24-1TH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, type of protection IP64",1305,"ΤΕΜ",1,"MC",1,"1FK70322AF241TH0"]
["1FK7032-2AF24-1TH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, type of protection IP65",1412,"ΤΕΜ",1,"MC",1,"1FK70322AF241TH1"]
["1FK7032-2AF24-1TH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.31 kW; UDC=300 V M0=1.2 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, degree of protection IP65 DE Flange IP67",1412,"ΤΕΜ",1,"MC",1,"1FK70322AF241TH2"]
["1FK7032-2AK71-1BA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP64",2104,"ΤΕΜ",1,"MC",1,"1FK70322AK711BA0"]
["1FK7032-2AK71-1BA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65",2212,"ΤΕΜ",1,"MC",1,"1FK70322AK711BA1"]
["1FK7032-2AK71-1BA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",2212,"ΤΕΜ",1,"MC",1,"1FK70322AK711BA2"]
["1FK7032-2AK71-1BB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP64",2356,"ΤΕΜ",1,"MC",1,"1FK70322AK711BB0"]
["1FK7032-2AK71-1BB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65",2463,"ΤΕΜ",1,"MC",1,"1FK70322AK711BB1"]
["1FK7032-2AK71-1BB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",2463,"ΤΕΜ",1,"MC",1,"1FK70322AK711BB2"]
["1FK7032-2AK71-1BG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP64",2005,"ΤΕΜ",1,"MC",1,"1FK70322AK711BG0"]
["1FK7032-2AK71-1BG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65",2113,"ΤΕΜ",1,"MC",1,"1FK70322AK711BG1"]
["1FK7032-2AK71-1BG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",2113,"ΤΕΜ",1,"MC",1,"1FK70322AK711BG2"]
["1FK7032-2AK71-1BH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP64",2254,"ΤΕΜ",1,"MC",1,"1FK70322AK711BH0"]
["1FK7032-2AK71-1BH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65",2361,"ΤΕΜ",1,"MC",1,"1FK70322AK711BH1"]
["1FK7032-2AK71-1BH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",2361,"ΤΕΜ",1,"MC",1,"1FK70322AK711BH2"]
["1FK7032-2AK71-1CA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP64",2528,"ΤΕΜ",1,"MC",1,"1FK70322AK711CA0"]
["1FK7032-2AK71-1CA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65",2635,"ΤΕΜ",1,"MC",1,"1FK70322AK711CA1"]
["1FK7032-2AK71-1CA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",2635,"ΤΕΜ",1,"MC",1,"1FK70322AK711CA2"]
["1FK7032-2AK71-1CB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP64",2779,"ΤΕΜ",1,"MC",1,"1FK70322AK711CB0"]
["1FK7032-2AK71-1CB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65",2887,"ΤΕΜ",1,"MC",1,"1FK70322AK711CB1"]
["1FK7032-2AK71-1CB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",2887,"ΤΕΜ",1,"MC",1,"1FK70322AK711CB2"]
["1FK7032-2AK71-1CG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP64",2429,"ΤΕΜ",1,"MC",1,"1FK70322AK711CG0"]
["1FK7032-2AK71-1CG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65",2537,"ΤΕΜ",1,"MC",1,"1FK70322AK711CG1"]
["1FK7032-2AK71-1CG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",2537,"ΤΕΜ",1,"MC",1,"1FK70322AK711CG2"]
["1FK7032-2AK71-1CH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP64",2678,"ΤΕΜ",1,"MC",1,"1FK70322AK711CH0"]
["1FK7032-2AK71-1CH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65",2785,"ΤΕΜ",1,"MC",1,"1FK70322AK711CH1"]
["1FK7032-2AK71-1CH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 24 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",2785,"ΤΕΜ",1,"MC",1,"1FK70322AK711CH2"]
["1FK7032-2AK71-1DA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2196,"ΤΕΜ",1,"MC",1,"1FK70322AK711DA0"]
["1FK7032-2AK71-1DA1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2302,"ΤΕΜ",1,"MC",1,"1FK70322AK711DA1"]
["1FK7032-2AK71-1DB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2448,"ΤΕΜ",1,"MC",1,"1FK70322AK711DB0"]
["1FK7032-2AK71-1DG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2097,"ΤΕΜ",1,"MC",1,"1FK70322AK711DG0"]
["1FK7032-2AK71-1DG1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2203,"ΤΕΜ",1,"MC",1,"1FK70322AK711DG1"]
["1FK7032-2AK71-1DG2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2203,"ΤΕΜ",1,"MC",1,"1FK70322AK711DG2"]
["1FK7032-2AK71-1DH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2346,"ΤΕΜ",1,"MC",1,"1FK70322AK711DH0"]
["1FK7032-2AK71-1DH1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2451,"ΤΕΜ",1,"MC",1,"1FK70322AK711DH1"]
["1FK7032-2AK71-1FA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2620,"ΤΕΜ",1,"MC",1,"1FK70322AK711FA0"]
["1FK7032-2AK71-1FA2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2725,"ΤΕΜ",1,"MC",1,"1FK70322AK711FA2"]
["1FK7032-2AK71-1FB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2871,"ΤΕΜ",1,"MC",1,"1FK70322AK711FB0"]
["1FK7032-2AK71-1FB1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2977,"ΤΕΜ",1,"MC",1,"1FK70322AK711FB1"]
["1FK7032-2AK71-1FG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2521,"ΤΕΜ",1,"MC",1,"1FK70322AK711FG0"]
["1FK7032-2AK71-1FG1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2626,"ΤΕΜ",1,"MC",1,"1FK70322AK711FG1"]
["1FK7032-2AK71-1FH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2770,"ΤΕΜ",1,"MC",1,"1FK70322AK711FH0"]
["1FK7032-2AK71-1FH1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2875,"ΤΕΜ",1,"MC",1,"1FK70322AK711FH1"]
["1FK7032-2AK71-1PA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP64",1432,"ΤΕΜ",1,"MC",1,"1FK70322AK711PA0"]
["1FK7032-2AK71-1PA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP65",1539,"ΤΕΜ",1,"MC",1,"1FK70322AK711PA1"]
["1FK7032-2AK71-1PA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1539,"ΤΕΜ",1,"MC",1,"1FK70322AK711PA2"]
["1FK7032-2AK71-1PB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP64",1683,"ΤΕΜ",1,"MC",1,"1FK70322AK711PB0"]
["1FK7032-2AK71-1PB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP65",1790,"ΤΕΜ",1,"MC",1,"1FK70322AK711PB1"]
["1FK7032-2AK71-1PB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1790,"ΤΕΜ",1,"MC",1,"1FK70322AK711PB2"]
["1FK7032-2AK71-1PG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP64",1333,"ΤΕΜ",1,"MC",1,"1FK70322AK711PG0"]
["1FK7032-2AK71-1PG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP65",1440,"ΤΕΜ",1,"MC",1,"1FK70322AK711PG1"]
["1FK7032-2AK71-1PG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1440,"ΤΕΜ",1,"MC",1,"1FK70322AK711PG2"]
["1FK7032-2AK71-1PH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP64",1581,"ΤΕΜ",1,"MC",1,"1FK70322AK711PH0"]
["1FK7032-2AK71-1PH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP65",1689,"ΤΕΜ",1,"MC",1,"1FK70322AK711PH1"]
["1FK7032-2AK71-1PH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1689,"ΤΕΜ",1,"MC",1,"1FK70322AK711PH2"]
["1FK7032-2AK71-1QA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP64",1550,"ΤΕΜ",1,"MC",1,"1FK70322AK711QA0"]
["1FK7032-2AK71-1QA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65",1657,"ΤΕΜ",1,"MC",1,"1FK70322AK711QA1"]
["1FK7032-2AK71-1QA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",1657,"ΤΕΜ",1,"MC",1,"1FK70322AK711QA2"]
["1FK7032-2AK71-1QB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP64",1801,"ΤΕΜ",1,"MC",1,"1FK70322AK711QB0"]
["1FK7032-2AK71-1QB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65",1909,"ΤΕΜ",1,"MC",1,"1FK70322AK711QB1"]
["1FK7032-2AK71-1QB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",1909,"ΤΕΜ",1,"MC",1,"1FK70322AK711QB2"]
["1FK7032-2AK71-1QG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP64",1451,"ΤΕΜ",1,"MC",1,"1FK70322AK711QG0"]
["1FK7032-2AK71-1QG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65",1558,"ΤΕΜ",1,"MC",1,"1FK70322AK711QG1"]
["1FK7032-2AK71-1QG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",1558,"ΤΕΜ",1,"MC",1,"1FK70322AK711QG2"]
["1FK7032-2AK71-1QH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP64",1700,"ΤΕΜ",1,"MC",1,"1FK70322AK711QH0"]
["1FK7032-2AK71-1QH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65",1807,"ΤΕΜ",1,"MC",1,"1FK70322AK711QH1"]
["1FK7032-2AK71-1QH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",1807,"ΤΕΜ",1,"MC",1,"1FK70322AK711QH2"]
["1FK7032-2AK71-1RA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP64",1979,"ΤΕΜ",1,"MC",1,"1FK70322AK711RA0"]
["1FK7032-2AK71-1RA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65",2087,"ΤΕΜ",1,"MC",1,"1FK70322AK711RA1"]
["1FK7032-2AK71-1RA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) Shaft with feather key, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",2087,"ΤΕΜ",1,"MC",1,"1FK70322AK711RA2"]
["1FK7032-2AK71-1RB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP64",2231,"ΤΕΜ",1,"MC",1,"1FK70322AK711RB0"]
["1FK7032-2AK71-1RB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65",2338,"ΤΕΜ",1,"MC",1,"1FK70322AK711RB1"]
["1FK7032-2AK71-1RB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) Shaft with feather key, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",2338,"ΤΕΜ",1,"MC",1,"1FK70322AK711RB2"]
["1FK7032-2AK71-1RG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP64",1880,"ΤΕΜ",1,"MC",1,"1FK70322AK711RG0"]
["1FK7032-2AK71-1RG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65",1988,"ΤΕΜ",1,"MC",1,"1FK70322AK711RG1"]
["1FK7032-2AK71-1RG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without Holding brake, degree of protection IP65 DE flange IP67",1988,"ΤΕΜ",1,"MC",1,"1FK70322AK711RG2"]
["1FK7032-2AK71-1RH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP64",2129,"ΤΕΜ",1,"MC",1,"1FK70322AK711RH0"]
["1FK7032-2AK71-1RH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65",2236,"ΤΕΜ",1,"MC",1,"1FK70322AK711RH1"]
["1FK7032-2AK71-1RH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable, absolute encoder 20 bit +12-bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with Holding brake, degree of protection IP65 DE flange IP67",2236,"ΤΕΜ",1,"MC",1,"1FK70322AK711RH2"]
["1FK7032-2AK71-1UA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP64",1432,"ΤΕΜ",1,"MC",1,"1FK70322AK711UA0"]
["1FK7032-2AK71-1UA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP65",1539,"ΤΕΜ",1,"MC",1,"1FK70322AK711UA1"]
["1FK7032-2AK71-1UA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1539,"ΤΕΜ",1,"MC",1,"1FK70322AK711UA2"]
["1FK7032-2AK71-1UB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP64",1683,"ΤΕΜ",1,"MC",1,"1FK70322AK711UB0"]
["1FK7032-2AK71-1UB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP65",1790,"ΤΕΜ",1,"MC",1,"1FK70322AK711UB1"]
["1FK7032-2AK71-1UB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1790,"ΤΕΜ",1,"MC",1,"1FK70322AK711UB2"]
["1FK7032-2AK71-1UG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP64",1333,"ΤΕΜ",1,"MC",1,"1FK70322AK711UG0"]
["1FK7032-2AK71-1UG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP65",1440,"ΤΕΜ",1,"MC",1,"1FK70322AK711UG1"]
["1FK7032-2AK71-1UG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1440,"ΤΕΜ",1,"MC",1,"1FK70322AK711UG2"]
["1FK7032-2AK71-1UH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP64",1581,"ΤΕΜ",1,"MC",1,"1FK70322AK711UH0"]
["1FK7032-2AK71-1UH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP65",1689,"ΤΕΜ",1,"MC",1,"1FK70322AK711UH1"]
["1FK7032-2AK71-1UH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1689,"ΤΕΜ",1,"MC",1,"1FK70322AK711UH2"]
["1FK7032-2AK74-1AA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1828,"ΤΕΜ",1,"MC",1,"1FK70322AK741AA0"]
["1FK7032-2AK74-1AA1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1933,"ΤΕΜ",1,"MC",1,"1FK70322AK741AA1"]
["1FK7032-2AK74-1AA2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1933,"ΤΕΜ",1,"MC",1,"1FK70322AK741AA2"]
["1FK7032-2AK74-1AB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2079,"ΤΕΜ",1,"MC",1,"1FK70322AK741AB0"]
["1FK7032-2AK74-1AB1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2184,"ΤΕΜ",1,"MC",1,"1FK70322AK741AB1"]
["1FK7032-2AK74-1AB2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2184,"ΤΕΜ",1,"MC",1,"1FK70322AK741AB2"]
["1FK7032-2AK74-1AG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1729,"ΤΕΜ",1,"MC",1,"1FK70322AK741AG0"]
["1FK7032-2AK74-1AG1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1834,"ΤΕΜ",1,"MC",1,"1FK70322AK741AG1"]
["1FK7032-2AK74-1AG2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1834,"ΤΕΜ",1,"MC",1,"1FK70322AK741AG2"]
["1FK7032-2AK74-1AH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1977,"ΤΕΜ",1,"MC",1,"1FK70322AK741AH0"]
["1FK7032-2AK74-1AH1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2082,"ΤΕΜ",1,"MC",1,"1FK70322AK741AH1"]
["1FK7032-2AK74-1AH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2082,"ΤΕΜ",1,"MC",1,"1FK70322AK741AH2"]
["1FK7032-2AK74-1EA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2254,"ΤΕΜ",1,"MC",1,"1FK70322AK741EA0"]
["1FK7032-2AK74-1EA1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2359,"ΤΕΜ",1,"MC",1,"1FK70322AK741EA1"]
["1FK7032-2AK74-1EA2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2359,"ΤΕΜ",1,"MC",1,"1FK70322AK741EA2"]
["1FK7032-2AK74-1EB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2505,"ΤΕΜ",1,"MC",1,"1FK70322AK741EB0"]
["1FK7032-2AK74-1EB1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2611,"ΤΕΜ",1,"MC",1,"1FK70322AK741EB1"]
["1FK7032-2AK74-1EB2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2611,"ΤΕΜ",1,"MC",1,"1FK70322AK741EB2"]
["1FK7032-2AK74-1EG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2155,"ΤΕΜ",1,"MC",1,"1FK70322AK741EG0"]
["1FK7032-2AK74-1EG1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2260,"ΤΕΜ",1,"MC",1,"1FK70322AK741EG1"]
["1FK7032-2AK74-1EG2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2260,"ΤΕΜ",1,"MC",1,"1FK70322AK741EG2"]
["1FK7032-2AK74-1EH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2404,"ΤΕΜ",1,"MC",1,"1FK70322AK741EH0"]
["1FK7032-2AK74-1EH1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2509,"ΤΕΜ",1,"MC",1,"1FK70322AK741EH1"]
["1FK7032-2AK74-1EH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.5kW; UDC=600V M0=1.15Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2509,"ΤΕΜ",1,"MC",1,"1FK70322AK741EH2"]
["1FK7032-2AK74-1SA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP64",1155,"ΤΕΜ",1,"MC",1,"1FK70322AK741SA0"]
["1FK7032-2AK74-1SA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP65",1263,"ΤΕΜ",1,"MC",1,"1FK70322AK741SA1"]
["1FK7032-2AK74-1SA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1263,"ΤΕΜ",1,"MC",1,"1FK70322AK741SA2"]
["1FK7032-2AK74-1SB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP64",1406,"ΤΕΜ",1,"MC",1,"1FK70322AK741SB0"]
["1FK7032-2AK74-1SB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP65",1514,"ΤΕΜ",1,"MC",1,"1FK70322AK741SB1"]
["1FK7032-2AK74-1SB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",1514,"ΤΕΜ",1,"MC",1,"1FK70322AK741SB2"]
["1FK7032-2AK74-1SG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP64",1056,"ΤΕΜ",1,"MC",1,"1FK70322AK741SG0"]
["1FK7032-2AK74-1SG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP65",1164,"ΤΕΜ",1,"MC",1,"1FK70322AK741SG1"]
["1FK7032-2AK74-1SG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP65 DE flange IP67",1164,"ΤΕΜ",1,"MC",1,"1FK70322AK741SG2"]
["1FK7032-2AK74-1SH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, type of protection IP64",1305,"ΤΕΜ",1,"MC",1,"1FK70322AK741SH0"]
["1FK7032-2AK74-1SH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, type of protection IP65",1412,"ΤΕΜ",1,"MC",1,"1FK70322AK741SH1"]
["1FK7032-2AK74-1SH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1412,"ΤΕΜ",1,"MC",1,"1FK70322AK741SH2"]
["1FK7032-2AK74-1TA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP64",1155,"ΤΕΜ",1,"MC",1,"1FK70322AK741TA0"]
["1FK7032-2AK74-1TA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP65",1263,"ΤΕΜ",1,"MC",1,"1FK70322AK741TA1"]
["1FK7032-2AK74-1TA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1263,"ΤΕΜ",1,"MC",1,"1FK70322AK741TA2"]
["1FK7032-2AK74-1TB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP64",1406,"ΤΕΜ",1,"MC",1,"1FK70322AK741TB0"]
["1FK7032-2AK74-1TB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP65",1514,"ΤΕΜ",1,"MC",1,"1FK70322AK741TB1"]
["1FK7032-2AK74-1TB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",1514,"ΤΕΜ",1,"MC",1,"1FK70322AK741TB2"]
["1FK7032-2AK74-1TG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP64",1056,"ΤΕΜ",1,"MC",1,"1FK70322AK741TG0"]
["1FK7032-2AK74-1TG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP65",1164,"ΤΕΜ",1,"MC",1,"1FK70322AK741TG1"]
["1FK7032-2AK74-1TG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N without holding brake, type of protection IP65 DE flange IP67",1164,"ΤΕΜ",1,"MC",1,"1FK70322AK741TG2"]
["1FK7032-2AK74-1TH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, type of protection IP64",1305,"ΤΕΜ",1,"MC",1,"1FK70322AK741TH0"]
["1FK7032-2AK74-1TH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, type of protection IP65",1412,"ΤΕΜ",1,"MC",1,"1FK70322AK741TH1"]
["1FK7032-2AK74-1TH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.5 kW; UDC=600V M0=1.15 Nm (100K); NN=6000rpm; naturally cooled IMB 5 design (IM V1, IM V3) flange 1, with Pt1000 Temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1412,"ΤΕΜ",1,"MC",1,"1FK70322AK741TH2"]
["1FK7033-4CF21-1BA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2155,"ΤΕΜ",1,"MC",1,"1FK70334CF211BA0"]
["1FK7033-4CF21-1BA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2260,"ΤΕΜ",1,"MC",1,"1FK70334CF211BA1"]
["1FK7033-4CF21-1BA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2260,"ΤΕΜ",1,"MC",1,"1FK70334CF211BA2"]
["1FK7033-4CF21-1BB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2406,"ΤΕΜ",1,"MC",1,"1FK70334CF211BB0"]
["1FK7033-4CF21-1BB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2512,"ΤΕΜ",1,"MC",1,"1FK70334CF211BB1"]
["1FK7033-4CF21-1BB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2512,"ΤΕΜ",1,"MC",1,"1FK70334CF211BB2"]
["1FK7033-4CF21-1BG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2056,"ΤΕΜ",1,"MC",1,"1FK70334CF211BG0"]
["1FK7033-4CF21-1BG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2161,"ΤΕΜ",1,"MC",1,"1FK70334CF211BG1"]
["1FK7033-4CF21-1BG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2161,"ΤΕΜ",1,"MC",1,"1FK70334CF211BG2"]
["1FK7033-4CF21-1BH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2305,"ΤΕΜ",1,"MC",1,"1FK70334CF211BH0"]
["1FK7033-4CF21-1BH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2410,"ΤΕΜ",1,"MC",1,"1FK70334CF211BH1"]
["1FK7033-4CF21-1BH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2410,"ΤΕΜ",1,"MC",1,"1FK70334CF211BH2"]
["1FK7033-4CF21-1CA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2579,"ΤΕΜ",1,"MC",1,"1FK70334CF211CA0"]
["1FK7033-4CF21-1CA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2684,"ΤΕΜ",1,"MC",1,"1FK70334CF211CA1"]
["1FK7033-4CF21-1CA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2684,"ΤΕΜ",1,"MC",1,"1FK70334CF211CA2"]
["1FK7033-4CF21-1CB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2830,"ΤΕΜ",1,"MC",1,"1FK70334CF211CB0"]
["1FK7033-4CF21-1CB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2935,"ΤΕΜ",1,"MC",1,"1FK70334CF211CB1"]
["1FK7033-4CF21-1CB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2935,"ΤΕΜ",1,"MC",1,"1FK70334CF211CB2"]
["1FK7033-4CF21-1CG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2480,"ΤΕΜ",1,"MC",1,"1FK70334CF211CG0"]
["1FK7033-4CF21-1CG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2585,"ΤΕΜ",1,"MC",1,"1FK70334CF211CG1"]
["1FK7033-4CF21-1CG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2585,"ΤΕΜ",1,"MC",1,"1FK70334CF211CG2"]
["1FK7033-4CF21-1CH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2728,"ΤΕΜ",1,"MC",1,"1FK70334CF211CH0"]
["1FK7033-4CF21-1CH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2834,"ΤΕΜ",1,"MC",1,"1FK70334CF211CH1"]
["1FK7033-4CF21-1CH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2834,"ΤΕΜ",1,"MC",1,"1FK70334CF211CH2"]
["1FK7033-4CF21-1DA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2247,"ΤΕΜ",1,"MC",1,"1FK70334CF211DA0"]
["1FK7033-4CF21-1DA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2352,"ΤΕΜ",1,"MC",1,"1FK70334CF211DA1"]
["1FK7033-4CF21-1DH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2502,"ΤΕΜ",1,"MC",1,"1FK70334CF211DH1"]
["1FK7033-4CF21-1PA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1483,"ΤΕΜ",1,"MC",1,"1FK70334CF211PA0"]
["1FK7033-4CF21-1PA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1588,"ΤΕΜ",1,"MC",1,"1FK70334CF211PA1"]
["1FK7033-4CF21-1PA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1588,"ΤΕΜ",1,"MC",1,"1FK70334CF211PA2"]
["1FK7033-4CF21-1PB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1734,"ΤΕΜ",1,"MC",1,"1FK70334CF211PB0"]
["1FK7033-4CF21-1PB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1839,"ΤΕΜ",1,"MC",1,"1FK70334CF211PB1"]
["1FK7033-4CF21-1PB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1839,"ΤΕΜ",1,"MC",1,"1FK70334CF211PB2"]
["1FK7033-4CF21-1PG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1384,"ΤΕΜ",1,"MC",1,"1FK70334CF211PG0"]
["1FK7033-4CF21-1PG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1489,"ΤΕΜ",1,"MC",1,"1FK70334CF211PG1"]
["1FK7033-4CF21-1PG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1489,"ΤΕΜ",1,"MC",1,"1FK70334CF211PG2"]
["1FK7033-4CF21-1PH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1632,"ΤΕΜ",1,"MC",1,"1FK70334CF211PH0"]
["1FK7033-4CF21-1PH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1737,"ΤΕΜ",1,"MC",1,"1FK70334CF211PH1"]
["1FK7033-4CF21-1PH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1737,"ΤΕΜ",1,"MC",1,"1FK70334CF211PH2"]
["1FK7033-4CF21-1QA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1601,"ΤΕΜ",1,"MC",1,"1FK70334CF211QA0"]
["1FK7033-4CF21-1QA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1706,"ΤΕΜ",1,"MC",1,"1FK70334CF211QA1"]
["1FK7033-4CF21-1QA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1706,"ΤΕΜ",1,"MC",1,"1FK70334CF211QA2"]
["1FK7033-4CF21-1QB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1852,"ΤΕΜ",1,"MC",1,"1FK70334CF211QB0"]
["1FK7033-4CF21-1QB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1957,"ΤΕΜ",1,"MC",1,"1FK70334CF211QB1"]
["1FK7033-4CF21-1QB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1957,"ΤΕΜ",1,"MC",1,"1FK70334CF211QB2"]
["1FK7033-4CF21-1QG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1502,"ΤΕΜ",1,"MC",1,"1FK70334CF211QG0"]
["1FK7033-4CF21-1QG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1607,"ΤΕΜ",1,"MC",1,"1FK70334CF211QG1"]
["1FK7033-4CF21-1QG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1607,"ΤΕΜ",1,"MC",1,"1FK70334CF211QG2"]
["1FK7033-4CF21-1QH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1750,"ΤΕΜ",1,"MC",1,"1FK70334CF211QH0"]
["1FK7033-4CF21-1QH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1856,"ΤΕΜ",1,"MC",1,"1FK70334CF211QH1"]
["1FK7033-4CF21-1QH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1856,"ΤΕΜ",1,"MC",1,"1FK70334CF211QH2"]
["1FK7033-4CF21-1RA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2030,"ΤΕΜ",1,"MC",1,"1FK70334CF211RA0"]
["1FK7033-4CF21-1RA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2135,"ΤΕΜ",1,"MC",1,"1FK70334CF211RA1"]
["1FK7033-4CF21-1RA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2135,"ΤΕΜ",1,"MC",1,"1FK70334CF211RA2"]
["1FK7033-4CF21-1RB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2281,"ΤΕΜ",1,"MC",1,"1FK70334CF211RB0"]
["1FK7033-4CF21-1RB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2387,"ΤΕΜ",1,"MC",1,"1FK70334CF211RB1"]
["1FK7033-4CF21-1RB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2387,"ΤΕΜ",1,"MC",1,"1FK70334CF211RB2"]
["1FK7033-4CF21-1RG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1931,"ΤΕΜ",1,"MC",1,"1FK70334CF211RG0"]
["1FK7033-4CF21-1RG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2036,"ΤΕΜ",1,"MC",1,"1FK70334CF211RG1"]
["1FK7033-4CF21-1RG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2036,"ΤΕΜ",1,"MC",1,"1FK70334CF211RG2"]
["1FK7033-4CF21-1RH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2180,"ΤΕΜ",1,"MC",1,"1FK70334CF211RH0"]
["1FK7033-4CF21-1RH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2285,"ΤΕΜ",1,"MC",1,"1FK70334CF211RH1"]
["1FK7033-4CF21-1RH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2285,"ΤΕΜ",1,"MC",1,"1FK70334CF211RH2"]
["1FK7033-4CF21-1UA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1483,"ΤΕΜ",1,"MC",1,"1FK70334CF211UA0"]
["1FK7033-4CF21-1UA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1588,"ΤΕΜ",1,"MC",1,"1FK70334CF211UA1"]
["1FK7033-4CF21-1UA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1588,"ΤΕΜ",1,"MC",1,"1FK70334CF211UA2"]
["1FK7033-4CF21-1UB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1734,"ΤΕΜ",1,"MC",1,"1FK70334CF211UB0"]
["1FK7033-4CF21-1UB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1839,"ΤΕΜ",1,"MC",1,"1FK70334CF211UB1"]
["1FK7033-4CF21-1UB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1839,"ΤΕΜ",1,"MC",1,"1FK70334CF211UB2"]
["1FK7033-4CF21-1UG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1384,"ΤΕΜ",1,"MC",1,"1FK70334CF211UG0"]
["1FK7033-4CF21-1UG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1489,"ΤΕΜ",1,"MC",1,"1FK70334CF211UG1"]
["1FK7033-4CF21-1UG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1489,"ΤΕΜ",1,"MC",1,"1FK70334CF211UG2"]
["1FK7033-4CF21-1UH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1632,"ΤΕΜ",1,"MC",1,"1FK70334CF211UH0"]
["1FK7033-4CF21-1UH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1737,"ΤΕΜ",1,"MC",1,"1FK70334CF211UH1"]
["1FK7033-4CF21-1UH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1737,"ΤΕΜ",1,"MC",1,"1FK70334CF211UH2"]
["1FK7033-4CF24-1AA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1984,"ΤΕΜ",1,"MC",1,"1FK70334CF241AA1"]
["1FK7033-4CF24-1AH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2028,"ΤΕΜ",1,"MC",1,"1FK70334CF241AH0"]
["1FK7033-4CF24-1EG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.38kW; UDC=300V; M0=1. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2206,"ΤΕΜ",1,"MC",1,"1FK70334CF241EG0"]
["1FK7033-4CK71-1BA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2155,"ΤΕΜ",1,"MC",1,"1FK70334CK711BA0"]
["1FK7033-4CK71-1BA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2260,"ΤΕΜ",1,"MC",1,"1FK70334CK711BA1"]
["1FK7033-4CK71-1BA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2260,"ΤΕΜ",1,"MC",1,"1FK70334CK711BA2"]
["1FK7033-4CK71-1BB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2406,"ΤΕΜ",1,"MC",1,"1FK70334CK711BB0"]
["1FK7033-4CK71-1BB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2512,"ΤΕΜ",1,"MC",1,"1FK70334CK711BB1"]
["1FK7033-4CK71-1BB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2512,"ΤΕΜ",1,"MC",1,"1FK70334CK711BB2"]
["1FK7033-4CK71-1BG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2056,"ΤΕΜ",1,"MC",1,"1FK70334CK711BG0"]
["1FK7033-4CK71-1BG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2161,"ΤΕΜ",1,"MC",1,"1FK70334CK711BG1"]
["1FK7033-4CK71-1BG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2161,"ΤΕΜ",1,"MC",1,"1FK70334CK711BG2"]
["1FK7033-4CK71-1BH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2305,"ΤΕΜ",1,"MC",1,"1FK70334CK711BH0"]
["1FK7033-4CK71-1BH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2410,"ΤΕΜ",1,"MC",1,"1FK70334CK711BH1"]
["1FK7033-4CK71-1BH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2410,"ΤΕΜ",1,"MC",1,"1FK70334CK711BH2"]
["1FK7033-4CK71-1CA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2579,"ΤΕΜ",1,"MC",1,"1FK70334CK711CA0"]
["1FK7033-4CK71-1CA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2684,"ΤΕΜ",1,"MC",1,"1FK70334CK711CA1"]
["1FK7033-4CK71-1CA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2684,"ΤΕΜ",1,"MC",1,"1FK70334CK711CA2"]
["1FK7033-4CK71-1CB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2830,"ΤΕΜ",1,"MC",1,"1FK70334CK711CB0"]
["1FK7033-4CK71-1CB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2935,"ΤΕΜ",1,"MC",1,"1FK70334CK711CB1"]
["1FK7033-4CK71-1CB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2935,"ΤΕΜ",1,"MC",1,"1FK70334CK711CB2"]
["1FK7033-4CK71-1CG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2480,"ΤΕΜ",1,"MC",1,"1FK70334CK711CG0"]
["1FK7033-4CK71-1CG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2585,"ΤΕΜ",1,"MC",1,"1FK70334CK711CG1"]
["1FK7033-4CK71-1CG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2585,"ΤΕΜ",1,"MC",1,"1FK70334CK711CG2"]
["1FK7033-4CK71-1CH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2728,"ΤΕΜ",1,"MC",1,"1FK70334CK711CH0"]
["1FK7033-4CK71-1CH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2834,"ΤΕΜ",1,"MC",1,"1FK70334CK711CH1"]
["1FK7033-4CK71-1CH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2834,"ΤΕΜ",1,"MC",1,"1FK70334CK711CH2"]
["1FK7033-4CK71-1DA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2247,"ΤΕΜ",1,"MC",1,"1FK70334CK711DA0"]
["1FK7033-4CK71-1DA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2352,"ΤΕΜ",1,"MC",1,"1FK70334CK711DA2"]
["1FK7033-4CK71-1DG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2148,"ΤΕΜ",1,"MC",1,"1FK70334CK711DG0"]
["1FK7033-4CK71-1PA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1483,"ΤΕΜ",1,"MC",1,"1FK70334CK711PA0"]
["1FK7033-4CK71-1PA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1588,"ΤΕΜ",1,"MC",1,"1FK70334CK711PA1"]
["1FK7033-4CK71-1PA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1588,"ΤΕΜ",1,"MC",1,"1FK70334CK711PA2"]
["1FK7033-4CK71-1PB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1734,"ΤΕΜ",1,"MC",1,"1FK70334CK711PB0"]
["1FK7033-4CK71-1PB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1839,"ΤΕΜ",1,"MC",1,"1FK70334CK711PB1"]
["1FK7033-4CK71-1PB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1839,"ΤΕΜ",1,"MC",1,"1FK70334CK711PB2"]
["1FK7033-4CK71-1PG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1384,"ΤΕΜ",1,"MC",1,"1FK70334CK711PG0"]
["1FK7033-4CK71-1PG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1489,"ΤΕΜ",1,"MC",1,"1FK70334CK711PG1"]
["1FK7033-4CK71-1PG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1489,"ΤΕΜ",1,"MC",1,"1FK70334CK711PG2"]
["1FK7033-4CK71-1PH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1632,"ΤΕΜ",1,"MC",1,"1FK70334CK711PH0"]
["1FK7033-4CK71-1PH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1737,"ΤΕΜ",1,"MC",1,"1FK70334CK711PH1"]
["1FK7033-4CK71-1PH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1737,"ΤΕΜ",1,"MC",1,"1FK70334CK711PH2"]
["1FK7033-4CK71-1QA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1601,"ΤΕΜ",1,"MC",1,"1FK70334CK711QA0"]
["1FK7033-4CK71-1QA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1706,"ΤΕΜ",1,"MC",1,"1FK70334CK711QA1"]
["1FK7033-4CK71-1QA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1706,"ΤΕΜ",1,"MC",1,"1FK70334CK711QA2"]
["1FK7033-4CK71-1QB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1852,"ΤΕΜ",1,"MC",1,"1FK70334CK711QB0"]
["1FK7033-4CK71-1QB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1957,"ΤΕΜ",1,"MC",1,"1FK70334CK711QB1"]
["1FK7033-4CK71-1QB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1957,"ΤΕΜ",1,"MC",1,"1FK70334CK711QB2"]
["1FK7033-4CK71-1QG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1502,"ΤΕΜ",1,"MC",1,"1FK70334CK711QG0"]
["1FK7033-4CK71-1QG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1607,"ΤΕΜ",1,"MC",1,"1FK70334CK711QG1"]
["1FK7033-4CK71-1QG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1607,"ΤΕΜ",1,"MC",1,"1FK70334CK711QG2"]
["1FK7033-4CK71-1QH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1750,"ΤΕΜ",1,"MC",1,"1FK70334CK711QH0"]
["1FK7033-4CK71-1QH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1856,"ΤΕΜ",1,"MC",1,"1FK70334CK711QH1"]
["1FK7033-4CK71-1QH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1856,"ΤΕΜ",1,"MC",1,"1FK70334CK711QH2"]
["1FK7033-4CK71-1RA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2030,"ΤΕΜ",1,"MC",1,"1FK70334CK711RA0"]
["1FK7033-4CK71-1RA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2135,"ΤΕΜ",1,"MC",1,"1FK70334CK711RA1"]
["1FK7033-4CK71-1RA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2135,"ΤΕΜ",1,"MC",1,"1FK70334CK711RA2"]
["1FK7033-4CK71-1RB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2281,"ΤΕΜ",1,"MC",1,"1FK70334CK711RB0"]
["1FK7033-4CK71-1RB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2387,"ΤΕΜ",1,"MC",1,"1FK70334CK711RB1"]
["1FK7033-4CK71-1RB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2387,"ΤΕΜ",1,"MC",1,"1FK70334CK711RB2"]
["1FK7033-4CK71-1RG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1931,"ΤΕΜ",1,"MC",1,"1FK70334CK711RG0"]
["1FK7033-4CK71-1RG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2036,"ΤΕΜ",1,"MC",1,"1FK70334CK711RG1"]
["1FK7033-4CK71-1RG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2036,"ΤΕΜ",1,"MC",1,"1FK70334CK711RG2"]
["1FK7033-4CK71-1RH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2180,"ΤΕΜ",1,"MC",1,"1FK70334CK711RH0"]
["1FK7033-4CK71-1RH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2285,"ΤΕΜ",1,"MC",1,"1FK70334CK711RH1"]
["1FK7033-4CK71-1RH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2285,"ΤΕΜ",1,"MC",1,"1FK70334CK711RH2"]
["1FK7033-4CK71-1UA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1483,"ΤΕΜ",1,"MC",1,"1FK70334CK711UA0"]
["1FK7033-4CK71-1UA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1588,"ΤΕΜ",1,"MC",1,"1FK70334CK711UA1"]
["1FK7033-4CK71-1UA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1588,"ΤΕΜ",1,"MC",1,"1FK70334CK711UA2"]
["1FK7033-4CK71-1UB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1734,"ΤΕΜ",1,"MC",1,"1FK70334CK711UB0"]
["1FK7033-4CK71-1UB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1839,"ΤΕΜ",1,"MC",1,"1FK70334CK711UB1"]
["1FK7033-4CK71-1UB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1839,"ΤΕΜ",1,"MC",1,"1FK70334CK711UB2"]
["1FK7033-4CK71-1UG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1384,"ΤΕΜ",1,"MC",1,"1FK70334CK711UG0"]
["1FK7033-4CK71-1UG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1489,"ΤΕΜ",1,"MC",1,"1FK70334CK711UG1"]
["1FK7033-4CK71-1UG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1489,"ΤΕΜ",1,"MC",1,"1FK70334CK711UG2"]
["1FK7033-4CK71-1UH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1632,"ΤΕΜ",1,"MC",1,"1FK70334CK711UH0"]
["1FK7033-4CK71-1UH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1737,"ΤΕΜ",1,"MC",1,"1FK70334CK711UH1"]
["1FK7033-4CK71-1UH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1737,"ΤΕΜ",1,"MC",1,"1FK70334CK711UH2"]
["1FK7033-4CK74-1AA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1878,"ΤΕΜ",1,"MC",1,"1FK70334CK741AA0"]
["1FK7033-4CK74-1AA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1984,"ΤΕΜ",1,"MC",1,"1FK70334CK741AA1"]
["1FK7033-4CK74-1AA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1984,"ΤΕΜ",1,"MC",1,"1FK70334CK741AA2"]
["1FK7033-4CK74-1AB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2130,"ΤΕΜ",1,"MC",1,"1FK70334CK741AB0"]
["1FK7033-4CK74-1AB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2235,"ΤΕΜ",1,"MC",1,"1FK70334CK741AB1"]
["1FK7033-4CK74-1AB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2235,"ΤΕΜ",1,"MC",1,"1FK70334CK741AB2"]
["1FK7033-4CK74-1AG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1780,"ΤΕΜ",1,"MC",1,"1FK70334CK741AG0"]
["1FK7033-4CK74-1AG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1885,"ΤΕΜ",1,"MC",1,"1FK70334CK741AG1"]
["1FK7033-4CK74-1AG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1885,"ΤΕΜ",1,"MC",1,"1FK70334CK741AG2"]
["1FK7033-4CK74-1AH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2028,"ΤΕΜ",1,"MC",1,"1FK70334CK741AH0"]
["1FK7033-4CK74-1AH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2133,"ΤΕΜ",1,"MC",1,"1FK70334CK741AH1"]
["1FK7033-4CK74-1AH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2133,"ΤΕΜ",1,"MC",1,"1FK70334CK741AH2"]
["1FK7033-4CK74-1EA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2305,"ΤΕΜ",1,"MC",1,"1FK70334CK741EA0"]
["1FK7033-4CK74-1EA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2410,"ΤΕΜ",1,"MC",1,"1FK70334CK741EA1"]
["1FK7033-4CK74-1EA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2410,"ΤΕΜ",1,"MC",1,"1FK70334CK741EA2"]
["1FK7033-4CK74-1EB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2556,"ΤΕΜ",1,"MC",1,"1FK70334CK741EB0"]
["1FK7033-4CK74-1EB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2661,"ΤΕΜ",1,"MC",1,"1FK70334CK741EB1"]
["1FK7033-4CK74-1EB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2661,"ΤΕΜ",1,"MC",1,"1FK70334CK741EB2"]
["1FK7033-4CK74-1EG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2206,"ΤΕΜ",1,"MC",1,"1FK70334CK741EG0"]
["1FK7033-4CK74-1EG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2311,"ΤΕΜ",1,"MC",1,"1FK70334CK741EG1"]
["1FK7033-4CK74-1EG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2311,"ΤΕΜ",1,"MC",1,"1FK70334CK741EG2"]
["1FK7033-4CK74-1EH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2454,"ΤΕΜ",1,"MC",1,"1FK70334CK741EH0"]
["1FK7033-4CK74-1EH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2560,"ΤΕΜ",1,"MC",1,"1FK70334CK741EH1"]
["1FK7033-4CK74-1EH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2560,"ΤΕΜ",1,"MC",1,"1FK70334CK741EH2"]
["1FK7033-4CK74-1SA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1206,"ΤΕΜ",1,"MC",1,"1FK70334CK741SA0"]
["1FK7033-4CK74-1SA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1311,"ΤΕΜ",1,"MC",1,"1FK70334CK741SA1"]
["1FK7033-4CK74-1SA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1311,"ΤΕΜ",1,"MC",1,"1FK70334CK741SA2"]
["1FK7033-4CK74-1SB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1457,"ΤΕΜ",1,"MC",1,"1FK70334CK741SB0"]
["1FK7033-4CK74-1SB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1562,"ΤΕΜ",1,"MC",1,"1FK70334CK741SB1"]
["1FK7033-4CK74-1SB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1562,"ΤΕΜ",1,"MC",1,"1FK70334CK741SB2"]
["1FK7033-4CK74-1SG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1107,"ΤΕΜ",1,"MC",1,"1FK70334CK741SG0"]
["1FK7033-4CK74-1SG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1212,"ΤΕΜ",1,"MC",1,"1FK70334CK741SG1"]
["1FK7033-4CK74-1SG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1212,"ΤΕΜ",1,"MC",1,"1FK70334CK741SG2"]
["1FK7033-4CK74-1SH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1355,"ΤΕΜ",1,"MC",1,"1FK70334CK741SH0"]
["1FK7033-4CK74-1SH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1461,"ΤΕΜ",1,"MC",1,"1FK70334CK741SH1"]
["1FK7033-4CK74-1SH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1461,"ΤΕΜ",1,"MC",1,"1FK70334CK741SH2"]
["1FK7033-4CK74-1TA0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1206,"ΤΕΜ",1,"MC",1,"1FK70334CK741TA0"]
["1FK7033-4CK74-1TA1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1311,"ΤΕΜ",1,"MC",1,"1FK70334CK741TA1"]
["1FK7033-4CK74-1TA2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1311,"ΤΕΜ",1,"MC",1,"1FK70334CK741TA2"]
["1FK7033-4CK74-1TB0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1457,"ΤΕΜ",1,"MC",1,"1FK70334CK741TB0"]
["1FK7033-4CK74-1TB1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1562,"ΤΕΜ",1,"MC",1,"1FK70334CK741TB1"]
["1FK7033-4CK74-1TB2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1562,"ΤΕΜ",1,"MC",1,"1FK70334CK741TB2"]
["1FK7033-4CK74-1TG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1107,"ΤΕΜ",1,"MC",1,"1FK70334CK741TG0"]
["1FK7033-4CK74-1TG1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",1212,"ΤΕΜ",1,"MC",1,"1FK70334CK741TG1"]
["1FK7033-4CK74-1TG2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",1212,"ΤΕΜ",1,"MC",1,"1FK70334CK741TG2"]
["1FK7033-4CK74-1TH0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1355,"ΤΕΜ",1,"MC",1,"1FK70334CK741TH0"]
["1FK7033-4CK74-1TH1","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",1461,"ΤΕΜ",1,"MC",1,"1FK70334CK741TH1"]
["1FK7033-4CK74-1TH2","SIMOTICS S Synchronous motor 1FK7-HD PN=0.57kW; UDC=600V M0=1. 3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1461,"ΤΕΜ",1,"MC",1,"1FK70334CK741TH2"]
["1FK7034-2AF21-1BA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",2214,"ΤΕΜ",1,"MC",1,"1FK70342AF211BA0"]
["1FK7034-2AF21-1BA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",2321,"ΤΕΜ",1,"MC",1,"1FK70342AF211BA1"]
["1FK7034-2AF21-1BA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",2321,"ΤΕΜ",1,"MC",1,"1FK70342AF211BA2"]
["1FK7034-2AF21-1BB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",2465,"ΤΕΜ",1,"MC",1,"1FK70342AF211BB0"]
["1FK7034-2AF21-1BB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",2572,"ΤΕΜ",1,"MC",1,"1FK70342AF211BB1"]
["1FK7034-2AF21-1BB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",2572,"ΤΕΜ",1,"MC",1,"1FK70342AF211BB2"]
["1FK7034-2AF21-1BG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",2115,"ΤΕΜ",1,"MC",1,"1FK70342AF211BG0"]
["1FK7034-2AF21-1BG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",2222,"ΤΕΜ",1,"MC",1,"1FK70342AF211BG1"]
["1FK7034-2AF21-1BG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",2222,"ΤΕΜ",1,"MC",1,"1FK70342AF211BG2"]
["1FK7034-2AF21-1BH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",2363,"ΤΕΜ",1,"MC",1,"1FK70342AF211BH0"]
["1FK7034-2AF21-1BH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",2470,"ΤΕΜ",1,"MC",1,"1FK70342AF211BH1"]
["1FK7034-2AF21-1BH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65, DE flange IP67",2470,"ΤΕΜ",1,"MC",1,"1FK70342AF211BH2"]
["1FK7034-2AF21-1CA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12- bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",2637,"ΤΕΜ",1,"MC",1,"1FK70342AF211CA0"]
["1FK7034-2AF21-1CA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",2745,"ΤΕΜ",1,"MC",1,"1FK70342AF211CA1"]
["1FK7034-2AF21-1CA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",2745,"ΤΕΜ",1,"MC",1,"1FK70342AF211CA2"]
["1FK7034-2AF21-1CB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",2889,"ΤΕΜ",1,"MC",1,"1FK70342AF211CB0"]
["1FK7034-2AF21-1CB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",2996,"ΤΕΜ",1,"MC",1,"1FK70342AF211CB1"]
["1FK7034-2AF21-1CB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",2996,"ΤΕΜ",1,"MC",1,"1FK70342AF211CB2"]
["1FK7034-2AF21-1CG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",2538,"ΤΕΜ",1,"MC",1,"1FK70342AF211CG0"]
["1FK7034-2AF21-1CG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",2646,"ΤΕΜ",1,"MC",1,"1FK70342AF211CG1"]
["1FK7034-2AF21-1CG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",2646,"ΤΕΜ",1,"MC",1,"1FK70342AF211CG2"]
["1FK7034-2AF21-1CH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",2787,"ΤΕΜ",1,"MC",1,"1FK70342AF211CH0"]
["1FK7034-2AF21-1CH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",2894,"ΤΕΜ",1,"MC",1,"1FK70342AF211CH1"]
["1FK7034-2AF21-1CH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65, DE flange IP67",2894,"ΤΕΜ",1,"MC",1,"1FK70342AF211CH2"]
["1FK7034-2AF21-1DA1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2413,"ΤΕΜ",1,"MC",1,"1FK70342AF211DA1"]
["1FK7034-2AF21-1DA2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2413,"ΤΕΜ",1,"MC",1,"1FK70342AF211DA2"]
["1FK7034-2AF21-1DB1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2664,"ΤΕΜ",1,"MC",1,"1FK70342AF211DB1"]
["1FK7034-2AF21-1DG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2207,"ΤΕΜ",1,"MC",1,"1FK70342AF211DG0"]
["1FK7034-2AF21-1DG2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2314,"ΤΕΜ",1,"MC",1,"1FK70342AF211DG2"]
["1FK7034-2AF21-1DH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2455,"ΤΕΜ",1,"MC",1,"1FK70342AF211DH0"]
["1FK7034-2AF21-1FB0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2981,"ΤΕΜ",1,"MC",1,"1FK70342AF211FB0"]
["1FK7034-2AF21-1FB2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3088,"ΤΕΜ",1,"MC",1,"1FK70342AF211FB2"]
["1FK7034-2AF21-1FG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2630,"ΤΕΜ",1,"MC",1,"1FK70342AF211FG0"]
["1FK7034-2AF21-1FG2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2738,"ΤΕΜ",1,"MC",1,"1FK70342AF211FG2"]
["1FK7034-2AF21-1FH0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2879,"ΤΕΜ",1,"MC",1,"1FK70342AF211FH0"]
["1FK7034-2AF21-1FH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2986,"ΤΕΜ",1,"MC",1,"1FK70342AF211FH2"]
["1FK7034-2AF21-1PA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP64",1541,"ΤΕΜ",1,"MC",1,"1FK70342AF211PA0"]
["1FK7034-2AF21-1PA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP65",1648,"ΤΕΜ",1,"MC",1,"1FK70342AF211PA1"]
["1FK7034-2AF21-1PA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1648,"ΤΕΜ",1,"MC",1,"1FK70342AF211PA2"]
["1FK7034-2AF21-1PB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP64",1792,"ΤΕΜ",1,"MC",1,"1FK70342AF211PB0"]
["1FK7034-2AF21-1PB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP65",1900,"ΤΕΜ",1,"MC",1,"1FK70342AF211PB1"]
["1FK7034-2AF21-1PB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1900,"ΤΕΜ",1,"MC",1,"1FK70342AF211PB2"]
["1FK7034-2AF21-1PG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP64",1442,"ΤΕΜ",1,"MC",1,"1FK70342AF211PG0"]
["1FK7034-2AF21-1PG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP65",1549,"ΤΕΜ",1,"MC",1,"1FK70342AF211PG1"]
["1FK7034-2AF21-1PG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1549,"ΤΕΜ",1,"MC",1,"1FK70342AF211PG2"]
["1FK7034-2AF21-1PH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP64",1690,"ΤΕΜ",1,"MC",1,"1FK70342AF211PH0"]
["1FK7034-2AF21-1PH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP65",1798,"ΤΕΜ",1,"MC",1,"1FK70342AF211PH1"]
["1FK7034-2AF21-1PH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1798,"ΤΕΜ",1,"MC",1,"1FK70342AF211PH2"]
["1FK7034-2AF21-1QA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",1659,"ΤΕΜ",1,"MC",1,"1FK70342AF211QA0"]
["1FK7034-2AF21-1QA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",1767,"ΤΕΜ",1,"MC",1,"1FK70342AF211QA1"]
["1FK7034-2AF21-1QA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1767,"ΤΕΜ",1,"MC",1,"1FK70342AF211QA2"]
["1FK7034-2AF21-1QB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",1911,"ΤΕΜ",1,"MC",1,"1FK70342AF211QB0"]
["1FK7034-2AF21-1QB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",2018,"ΤΕΜ",1,"MC",1,"1FK70342AF211QB1"]
["1FK7034-2AF21-1QB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",2018,"ΤΕΜ",1,"MC",1,"1FK70342AF211QB2"]
["1FK7034-2AF21-1QG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",1560,"ΤΕΜ",1,"MC",1,"1FK70342AF211QG0"]
["1FK7034-2AF21-1QG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",1668,"ΤΕΜ",1,"MC",1,"1FK70342AF211QG1"]
["1FK7034-2AF21-1QG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",1668,"ΤΕΜ",1,"MC",1,"1FK70342AF211QG2"]
["1FK7034-2AF21-1QH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",1809,"ΤΕΜ",1,"MC",1,"1FK70342AF211QH0"]
["1FK7034-2AF21-1QH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",1916,"ΤΕΜ",1,"MC",1,"1FK70342AF211QH1"]
["1FK7034-2AF21-1QH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65, DE flange IP67",1916,"ΤΕΜ",1,"MC",1,"1FK70342AF211QH2"]
["1FK7034-2AF21-1RA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",2089,"ΤΕΜ",1,"MC",1,"1FK70342AF211RA0"]
["1FK7034-2AF21-1RA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65",2196,"ΤΕΜ",1,"MC",1,"1FK70342AF211RA1"]
["1FK7034-2AF21-1RA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",2196,"ΤΕΜ",1,"MC",1,"1FK70342AF211RA2"]
["1FK7034-2AF21-1RB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",2340,"ΤΕΜ",1,"MC",1,"1FK70342AF211RB0"]
["1FK7034-2AF21-1RB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65",2447,"ΤΕΜ",1,"MC",1,"1FK70342AF211RB1"]
["1FK7034-2AF21-1RB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",2447,"ΤΕΜ",1,"MC",1,"1FK70342AF211RB2"]
["1FK7034-2AF21-1RG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without holding brake degree of protection IP64",1990,"ΤΕΜ",1,"MC",1,"1FK70342AF211RG0"]
["1FK7034-2AF21-1RG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",2097,"ΤΕΜ",1,"MC",1,"1FK70342AF211RG1"]
["1FK7034-2AF21-1RG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N without holding brake degree of protection IP65, DE flange IP67",2097,"ΤΕΜ",1,"MC",1,"1FK70342AF211RG2"]
["1FK7034-2AF21-1RH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with holding brake degree of protection IP64",2238,"ΤΕΜ",1,"MC",1,"1FK70342AF211RH0"]
["1FK7034-2AF21-1RH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",2345,"ΤΕΜ",1,"MC",1,"1FK70342AF211RH1"]
["1FK7034-2AF21-1RH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65, DE flange IP67",2345,"ΤΕΜ",1,"MC",1,"1FK70342AF211RH2"]
["1FK7034-2AF21-1UA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP64",1541,"ΤΕΜ",1,"MC",1,"1FK70342AF211UA0"]
["1FK7034-2AF21-1UA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP65",1648,"ΤΕΜ",1,"MC",1,"1FK70342AF211UA1"]
["1FK7034-2AF21-1UA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1648,"ΤΕΜ",1,"MC",1,"1FK70342AF211UA2"]
["1FK7034-2AF21-1UB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP64",1792,"ΤΕΜ",1,"MC",1,"1FK70342AF211UB0"]
["1FK7034-2AF21-1UB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, type of protection IP65",1900,"ΤΕΜ",1,"MC",1,"1FK70342AF211UB1"]
["1FK7034-2AF21-1UB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1900,"ΤΕΜ",1,"MC",1,"1FK70342AF211UB2"]
["1FK7034-2AF21-1UG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP64",1442,"ΤΕΜ",1,"MC",1,"1FK70342AF211UG0"]
["1FK7034-2AF21-1UG1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, type of protection IP65",1549,"ΤΕΜ",1,"MC",1,"1FK70342AF211UG1"]
["1FK7034-2AF21-1UG2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake, degree of protection IP65 DE flange IP67",1549,"ΤΕΜ",1,"MC",1,"1FK70342AF211UG2"]
["1FK7034-2AF21-1UH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP64",1690,"ΤΕΜ",1,"MC",1,"1FK70342AF211UH0"]
["1FK7034-2AF21-1UH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, type of protection IP65",1798,"ΤΕΜ",1,"MC",1,"1FK70342AF211UH1"]
["1FK7034-2AF21-1UH2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake, degree of protection IP65 DE flange IP67",1798,"ΤΕΜ",1,"MC",1,"1FK70342AF211UH2"]
["1FK7034-2AF24-1EG0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.47kW; UDC=300V; M0=1.6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2264,"ΤΕΜ",1,"MC",1,"1FK70342AF241EG0"]
["1FK7034-2AF24-1SA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP64",1264,"ΤΕΜ",1,"MC",1,"1FK70342AF241SA0"]
["1FK7034-2AF24-1SA1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP65",1372,"ΤΕΜ",1,"MC",1,"1FK70342AF241SA1"]
["1FK7034-2AF24-1SA2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N without holding brake degree of protection IP65, DE flange IP67",1372,"ΤΕΜ",1,"MC",1,"1FK70342AF241SA2"]
["1FK7034-2AF24-1SB0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP64",1516,"ΤΕΜ",1,"MC",1,"1FK70342AF241SB0"]
["1FK7034-2AF24-1SB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP65",1623,"ΤΕΜ",1,"MC",1,"1FK70342AF241SB1"]
["1FK7034-2AF24-1SB2","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",1623,"ΤΕΜ",1,"MC",1,"1FK70342AF241SB2"]
["1FK7034-2AF24-1SG0","SIMOTICS S synchronous motor 1FK7-CT PN=0.47 kW; UDC=300 V M0=1.6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=3) smooth shaft, tolerance N without holding brake, type of protection IP64",1165,"ΤΕΜ",1,"MC",1,"1FK70342AF241SG0"]
["1FK7034-2AK71-1FH2","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",2984,"ΤΕΜ",1,"MC",1,"1FK70342AK711FH2"]
["1FK7034-2AK74-1AA0","SIMOTICS S Synchronous motor 1FK7-CT PN=0.63kW; UDC=600V M0=1.6Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1937,"ΤΕΜ",1,"MC",1,"1FK70342AK741AA0"]
["1FK7040-2AK74-1TH0","SIMOTICS S synchronous motor 1FK7-CT PN=0.69 kW; UDC=600V M0=1.6 Nm (100K); NN=6000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) smooth shaft, tolerance N with holding brake, type of protection IP64",1427,"ΤΕΜ",1,"MC",1,"1FK70402AK741TH0"]
["1FK7042-2AC71-1DG1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.59kW; UDC=600V M0=3Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2350,"ΤΕΜ",1,"MC",1,"1FK70422AC711DG1"]
["1FK7042-2AC74-1TA0","SIMOTICS S synchronous motor 1FK7-CT PN=0.59 kW; UDC=600V M0=3Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP64",1302,"ΤΕΜ",1,"MC",1,"1FK70422AC741TA0"]
["1FK7042-2AF21-1UB1","SIMOTICS S synchronous motor 1FK7-CT PN=0.82 kW; UDC=300 V M0=3 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake degree of protection IP65",1986,"ΤΕΜ",1,"MC",1,"1FK70422AF211UB1"]
["1FK7042-2AF74-1TB2","SIMOTICS S SIMOTICS S-1FK7 synchronous motor 1FK7-CT PN=0.82 kW; UDC=600 V M0=3 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N with holding brake degree of protection IP65, DE flange IP67",1709,"ΤΕΜ",1,"MC",1,"1FK70422AF741TB2"]
["1FK7042-2AK71-1PH1","SIMOTICS S synchronous motor 1FK7-CT PN=0.94 kW; UDC=600 V M0=3 Nm (100K); NN=6000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake degree of protection IP65",1884,"ΤΕΜ",1,"MC",1,"1FK70422AK711PH1"]
["1FK7042-2AK74-1AH1","SIMOTICS S Synchronous motor 1FK7-CT PN=0.94kW; UDC=600V M0=3Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2278,"ΤΕΜ",1,"MC",1,"1FK70422AK741AH1"]
["1FK7043-4CF21-1RG0","SIMOTICS S Synchronous motor 1FK7-HD PN=0.94kW; UDC=300V; M0=3. 3Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2078,"ΤΕΜ",1,"MC",1,"1FK70434CF211RG0"]
["1FK7043-4CH71-1FH0","SIMOTICS S Synchronous motor 1FK7-HD PN=1.2kW; UDC=600V M0=3.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3016,"ΤΕΜ",1,"MC",1,"1FK70434CH711FH0"]
["1FK7043-4CH74-1SH2","SIMOTICS S Synchronous motor 1FK7-HD PN=1.2kW; UDC=600V M0=3.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1656,"ΤΕΜ",1,"MC",1,"1FK70434CH741SH2"]
["1FK7043-4CK71-1UG0","SIMOTICS S Synchronous motor 1FK7-HD PN=1.3kW; UDC=600V M0=3.5Nm (100K); NN=6000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1531,"ΤΕΜ",1,"MC",1,"1FK70434CK711UG0"]
["1FK7044-4CF74-1TH2","SIMOTICS S Synchronous motor 1FK7-HD PN=1.2kW; UDC=600V M0=4.5Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",1737,"ΤΕΜ",1,"MC",1,"1FK70444CF741TH2"]
["1FK7044-4CH71-1QA0","SIMOTICS S Synchronous motor 1FK7-HD PN=1.4kW; UDC=600V M0=4.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",1829,"ΤΕΜ",1,"MC",1,"1FK70444CH711QA0"]
["1FK7044-4CH74-1TH0","SIMOTICS S Synchronous motor 1FK7-HD PN=1.4kW; UDC=600V M0=4.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",1632,"ΤΕΜ",1,"MC",1,"1FK70444CH741TH0"]
["1FK7060-2AC71-1RA2","SIMOTICS S Synchronous motor 1FK7-CT PN=1.1kW; UDC=600V M0=6Nm (100K); NN=2000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 20-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N without holding brake IP65 degree of protection DE flange IP67",2480,"ΤΕΜ",1,"MC",1,"1FK70602AC711RA2"]
["1FK7060-2AF71-1UB2","SIMOTICS S synchronous motor 1FK7-CT PN=1.5 kW; UDC=600 V M0=6 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake degree of protection IP65 DE flange IP67",2280,"ΤΕΜ",1,"MC",1,"1FK70602AF711UB2"]
["1FK7060-2AH71-1CH2","SIMOTICS S synchronous motor 1FK7-CT PN=1.7 kW; UDC=600 V M0=6 Nm (100K); NN=4500 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12- bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) smooth shaft, tolerance N with holding brake degree of protection IP65 DE flange IP67",3280,"ΤΕΜ",1,"MC",1,"1FK70602AH711CH2"]
["1FK7060-3BF71-1FH1","SIMOTICS S Synchronous motor 1FK7-HI PN=1.5kW; UDC=600V M0=6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",3370,"ΤΕΜ",1,"MC",1,"1FK70603BF711FH1"]
["1FK7060-3BF74-1EG1","SIMOTICS S Synchronous motor 1FK7-HI PN=1.5kW; UDC=600V M0=6Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2654,"ΤΕΜ",1,"MC",1,"1FK70603BF741EG1"]
["1FK7061-4CF74-1AA1","SIMOTICS S Synchronous motor 1FK7-HD PN=1.7kW; UDC=600V M0=6.4Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",2453,"ΤΕΜ",1,"MC",1,"1FK70614CF741AA1"]
["1FK7061-4CH71-1PH1","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=6.4Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",2309,"ΤΕΜ",1,"MC",1,"1FK70614CH711PH1"]
["1FK7062-2AC71-1BA1","SIMOTICS S synchronous motor 1FK7-CT PN=1.5kW; UDC=600V M0=8.5Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N without holding brake, degree of protection IP65",2754,"ΤΕΜ",1,"MC",1,"1FK70622AC711BA1"]
["1FK7062-2AF71-1BG1","SIMOTICS S synchronous motor 1FK7-CT PN=1.9 kW; UDC=600 V M0=8.5 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 24-bit with DRIVE-CLiQ interface (encoder AS24DQI) smooth shaft, tolerance N without holding brake degree of protection IP65",2655,"ΤΕΜ",1,"MC",1,"1FK70622AF711BG1"]
["1FK7062-2AF74-1AB2","SIMOTICS S Synchronous motor 1FK7-CT PN=1.9kW; UDC=600V M0=8.5Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2825,"ΤΕΜ",1,"MC",1,"1FK70622AF741AB2"]
["1FK7062-2AH74-1AH0","SIMOTICS S Synchronous motor 1FK7-CT PN=1.4kW; UDC=600V M0=8.5Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2621,"ΤΕΜ",1,"MC",1,"1FK70622AH741AH0"]
["1FK7062-3BF71-1RB2","SIMOTICS S synchronous motor 1FK7-HI PN=1.9 kW; UDC=600 V M0=8.5 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 20-bit +12- bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65 DE flange IP67",2977,"ΤΕΜ",1,"MC",1,"1FK70623BF711RB2"]
["1FK7063-2AC71-1QA1","SIMOTICS S synchronous motor 1FK7-CT PN=1.9kW; UDC=600V M0=11Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake, degree of protection IP65",2307,"ΤΕΜ",1,"MC",1,"1FK70632AC711QA1"]
["1FK7063-2AC74-1EA2","SIMOTICS S Synchronous motor 1FK7-CT PN=1.9kW; UDC=600V M0=11Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",3009,"ΤΕΜ",1,"MC",1,"1FK70632AC741EA2"]
["1FK7063-2AF74-1AH0","SIMOTICS S Synchronous motor 1FK7-CT PN=2.3kW; UDC=600V M0=11Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",2729,"ΤΕΜ",1,"MC",1,"1FK70632AF741AH0"]
["1FK7063-2AH74-1AA2","SIMOTICS S Synchronous motor 1FK7-CT PN=1.4kW; UDC=600V M0=11Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",2583,"ΤΕΜ",1,"MC",1,"1FK70632AH741AA2"]
["1FK7064-4CC71-1BB0","SIMOTICS S Synchronous motor 1FK7-HD PN=2.1kW; UDC=600V M0=12Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3284,"ΤΕΜ",1,"MC",1,"1FK70644CC711BB0"]
["1FK7064-4CC74-1EA1","SIMOTICS S Synchronous motor 1FK7-HD PN=2.1kW; UDC=600V M0=12Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",3192,"ΤΕΜ",1,"MC",1,"1FK70644CC741EA1"]
["1FK7064-4CH71-1CA1","SIMOTICS S Synchronous motor 1FK7-HD PN=2.4kW; UDC=600V M0=12Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",3466,"ΤΕΜ",1,"MC",1,"1FK70644CH711CA1"]
["1FK7064-4CH71-1RH0","SIMOTICS S Synchronous motor 1FK7-HD PN=2.4kW; UDC=600V M0=12Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3063,"ΤΕΜ",1,"MC",1,"1FK70644CH711RH0"]
["1FK7080-2AF71-1RB2","SIMOTICS S synchronous motor 1FK7-CT PN=2.1 kW; UDC=600 V M0=8 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 20-bit +12- bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake degree of protection IP65 DE flange IP67",3148,"ΤΕΜ",1,"MC",1,"1FK70802AF711RB2"]
["1FK7080-2AH71-1PB1","SIMOTICS S synchronous motor 1FK7-CT PN=2.1 kW; UDC=600 V M0=8 Nm (100K); NN=4500 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake degree of protection IP65",2600,"ΤΕΜ",1,"MC",1,"1FK70802AH711PB1"]
["1FK7080-2AH74-1TA1","SIMOTICS S synchronous motor 1FK7-CT PN=2.1 kW; UDC=600V M0=8Nm (100K); NN=4500rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable 2-pole resolver (resolver P=1) shaft with feather key, tolerance N without holding brake degree of protection IP65",1851,"ΤΕΜ",1,"MC",1,"1FK70802AH741TA1"]
["1FK7081-2AC71-1UA1","SIMOTICS S synchronous motor 1FK7-CT PN=2.1 kW; UDC=600V M0=12Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake, type of protection IP65",2377,"ΤΕΜ",1,"MC",1,"1FK70812AC711UA1"]
["1FK7081-2AF71-1PH1","SIMOTICS S synchronous motor 1FK7-CT PN=2.7 kW; UDC=600 V M0=12 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake degree of protection IP65",2751,"ΤΕΜ",1,"MC",1,"1FK70812AF711PH1"]
["1FK7081-2AH71-1QA0","SIMOTICS S synchronous motor 1FK7-CT PN=1.8 kW; UDC=600V M0=12Nm (100K); NN=4500rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder single-turn 20-bit with DRIVE-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N without holding brake degree of protection IP64",2388,"ΤΕΜ",1,"MC",1,"1FK70812AH711QA0"]
["1FK7081-2AH74-1EA1","SIMOTICS S Synchronous motor 1FK7-CT PN=1.8kW; UDC=600V M0=12Nm (100K); NN=4500rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",3200,"ΤΕΜ",1,"MC",1,"1FK70812AH741EA1"]
["1FK7081-3BF71-1QG0","SIMOTICS S synchronous motor 1FK7-HI PN=2.7kW; UDC=600V M0=12Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) Smooth shaft, tolerance N without holding brake, degree of protection IP64",2290,"ΤΕΜ",1,"MC",1,"1FK70813BF711QG0"]
["1FK7083-2AC71-1PG0","SIMOTICS S synchronous motor 1FK7-CT PN=2.6 kW; UDC=600 V M0=16 Nm (100K); NN=2000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N without holding brake degree of protection IP64",2295,"ΤΕΜ",1,"MC",1,"1FK70832AC711PG0"]
["1FK7083-2AF71-1PH1","SIMOTICS S synchronous motor 1FK7-CT PN=3.3 kW; UDC=600 V M0=16 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake degree of protection IP65",2874,"ΤΕΜ",1,"MC",1,"1FK70832AF711PH1"]
["1FK7083-2AH71-1PA1","SIMOTICS S synchronous motor 1FK7-CT PN=1.4 kW; UDC=600 V M0=16 Nm (100K); NN=4500 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface shaft with feather key, tolerance N without holding brake degree of protection IP65",2501,"ΤΕΜ",1,"MC",1,"1FK70832AH711PA1"]
["1FK7083-2AH71-1UB0","SIMOTICS S synchronous motor 1FK7-CT PN=1.4 kW; UDC=600 V M0=16 Nm (100K); NN=4500 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable multi-pole resolver with DRIVE-CLiQ interface shaft with feather key, tolerance N with holding brake degree of protection IP64",2866,"ΤΕΜ",1,"MC",1,"1FK70832AH711UB0"]
["1FK7084-2AC74-1AA0","SIMOTICS S Synchronous motor 1FK7-CT PN=3.1kW; UDC=600V M0=20Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3131,"ΤΕΜ",1,"MC",1,"1FK70842AC741AA0"]
["1FK7084-2AF71-1FG1","SIMOTICS S Synchronous motor 1FK7-CT PN=3.1kW; UDC=600V M0=20Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65",3930,"ΤΕΜ",1,"MC",1,"1FK70842AF711FG1"]
["1FK7084-3BC71-1BA1","SIMOTICS S synchronous motor 1FK7-HI PN=3.1kW; UDC=600V M0=20Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) shaft with feather key, tolerance N without holding brake, degree of protection IP65",3515,"ΤΕΜ",1,"MC",1,"1FK70843BC711BA1"]
["1FK7084-3BF71-1FB1","SIMOTICS S Synchronous motor 1FK7-HI PN=3.1kW; UDC=600V M0=20Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",4503,"ΤΕΜ",1,"MC",1,"1FK70843BF711FB1"]
["1FK7085-4CC71-1PA2","SIMOTICS S Synchronous motor 1FK7-HD PN=3.1kW; UDC=600V M0=22Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",3001,"ΤΕΜ",1,"MC",1,"1FK70854CC711PA2"]
["1FK7085-4CC74-1AA0","SIMOTICS S Synchronous motor 1FK7-HD PN=3.1kW; UDC=600V M0=22Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",3292,"ΤΕΜ",1,"MC",1,"1FK70854CC741AA0"]
["1FK7085-4CF71-1PG0","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=22Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",2797,"ΤΕΜ",1,"MC",1,"1FK70854CF711PG0"]
["1FK7086-4CC71-1RB1","SIMOTICS S Synchronous motor 1FK7-HD PN=3.8kW; UDC=600V M0=28Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",4478,"ΤΕΜ",1,"MC",1,"1FK70864CC711RB1"]
["1FK7086-4CF71-1RB0","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=28Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",4373,"ΤΕΜ",1,"MC",1,"1FK70864CF711RB0"]
["1FK7086-4CF74-1EG2","SIMOTICS S Synchronous motor 1FK7-HD PN=2kW; UDC=600V M0=28Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP65 DE flange IP67",4182,"ΤΕΜ",1,"MC",1,"1FK70864CF741EG2"]
["1FK7100-2AC74-1EB0","SIMOTICS S Synchronous motor 1FK7-CT PN=3kW; UDC=600V M0=18Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP64",3972,"ΤΕΜ",1,"MC",1,"1FK71002AC741EB0"]
["1FK7100-2AF71-1PH2","SIMOTICS S synchronous motor 1FK7-CT PN=3.8 kW; UDC=600 V M0=18 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable 2-pole resolver, with DRIVE-CLiQ interface smooth shaft, tolerance N with holding brake degree of protection IP65 DE flange IP67",3158,"ΤΕΜ",1,"MC",1,"1FK71002AF711PH2"]
["1FK7100-2AF74-1SA0","SIMOTICS S synchronous motor 1FK7-CT PN=3.8 kW; UDC=600V M0=18Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=4) shaft with feather key, tolerance N without holding brake degree of protection IP64",2401,"ΤΕΜ",1,"MC",1,"1FK71002AF741SA0"]
["1FK7100-3BC71-1RH1","SIMOTICS S synchronous motor 1FK7-HI PN=3 kW; UDC=600V M0=18Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable Absolute encoder 20-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM20DQI) smooth shaft, tolerance N with holding brake degree of protection IP65",3696,"ΤΕΜ",1,"MC",1,"1FK71003BC711RH1"]
["1FK7101-2AF71-1CA1","SIMOTICS S synchronous motor 1FK7-CT PN=4.9kW; UDC=600V M0=27Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit + 12-bit multiturn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N without holding brake, degree of protection IP65",4249,"ΤΕΜ",1,"MC",1,"1FK71012AF711CA1"]
["1FK7101-2AF71-1QB2","SIMOTICS S synchronous motor 1FK7-CT PN=4.9kW; UDC=600V M0=27Nm (100K); NN=3000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake, degree of protection IP65 DE Flange, IP67",3744,"ΤΕΜ",1,"MC",1,"1FK71012AF711QB2"]
["1FK7101-3BC71-1BG2","SIMOTICS S synchronous motor 1FK7-HI PN=4.3kW; UDC=600V M0=27Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 24-bit with Drive-CLiQ interface (encoder AS24DQI) Smooth shaft, tolerance N without holding brake, degree of protection IP65 DE Flange, IP67",3712,"ΤΕΜ",1,"MC",1,"1FK71013BC711BG2"]
["1FK7101-3BF71-1CB0","SIMOTICS S synchronous motor 1FK7-HI PN=4.9 kW; UDC=600V M0=27 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1 power connector rotatable absolute encoder 24-bit +12 bit multi-turn with DRIVE-CLiQ interface (encoder AM24DQI) shaft with feather key, tolerance N with holding brake degree of protection IP64",4600,"ΤΕΜ",1,"MC",1,"1FK71013BF711CB0"]
["1FK7103-2AC74-1AB2","SIMOTICS S Synchronous motor 1FK7-CT PN=5.2kW; UDC=600V M0=36Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65 DE flange IP67",4504,"ΤΕΜ",1,"MC",1,"1FK71032AC741AB2"]
["1FK7103-2AF71-1RB1","SIMOTICS S Synchronous motor 1FK7-CT PN=4.4kW; UDC=600V M0=36Nm (100K); NN=3000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 20-bit +12-bit multi-turn with Drive-CLiQ interface (encoder AM20DQI) shaft with feather key, tolerance N with holding brake IP65 degree of protection",4658,"ΤΕΜ",1,"MC",1,"1FK71032AF711RB1"]
["1FK7103-2AF74-1SG2","SIMOTICS S synchronous motor 1FK7-CT PN=4.4 kW; UDC=600V M0=36 Nm (100K); NN=3000 rpm; naturally cooled design IMB 5 (IM V1, IM V3) flange 1, with Pt1000 temperature sensor power connector rotatable multi-pole resolver (resolver P=4) smooth shaft, tolerance N without holding brake, type of protection IP65 DE flange IP67",3262,"ΤΕΜ",1,"MC",1,"1FK71032AF741SG2"]
["1FK7103-3BF74-1AG1","SIMOTICS S Synchronous motor 1FK7-HI PN=4.4kW; UDC=600V M0=36Nm (100K); NN=3000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VP 2048 S/R WITH C- AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",3915,"ΤΕΜ",1,"MC",1,"1FK71033BF741AG1"]
["1FK7105-2AC71-1FH1","SIMOTICS S Synchronous motor 1FK7-CT PN=7.7kW; UDC=600V M0=48Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE Degree of protection IP65",6415,"ΤΕΜ",1,"MC",1,"1FK71052AC711FH1"]
["1FK7105-2AC74-1GG0","SIMOTICS S Synchronous motor 1FK7-CT PN=7.7kW; UDC=600V M0=48Nm (100K); NN=2000rpm; Naturally cooled FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH PT1000 TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 32 S/R SINGLETURN, 4096 ROTATION MULTITURN, WITH ENDAT- INTERFACE (ENCODER AM32S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE Degree of protection IP64",4878,"ΤΕΜ",1,"MC",1,"1FK71052AC741GG0"]
["1FK7105-2AF71-1QB0","SIMOTICS S Synchronous motor 1FK7-CT PN=8.2kW; UDC=600V M0=48Nm (100K); NN=3000rpm; Naturally cooled IMB 5 design (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder single-turn 20-bit with Drive-CLiQ interface (encoder AS20DQI) shaft with feather key, tolerance N with holding brake IP64 degree of protection",5339,"ΤΕΜ",1,"MC",1,"1FK71052AF711QB0"]
["1FK7105-3BC71-1CG2","SIMOTICS S synchronous motor 1FK7-HI PN=7.7kW; UDC=600V M0=48Nm (100K); NN=2000rpm; naturally cooled design IMB 5 (IM V1, IM V3) Flange 1 Power connector rotatable Absolute encoder 24-bit + 12-bit multiturn with DRIVE-CLiQ interface (encoder AM24DQI) Smooth shaft, tolerance N without holding brake, degree of protection IP65 DE Flange, IP67",5824,"ΤΕΜ",1,"MC",1,"1FK71053BC711CG2"]
["1FL6044-1AF61-2LG1","SIMOTICS S-1FL6 Operating voltage 3AC 400 V Pn=0.75 kW; Nn=3000 rpm M0=3.5 Nm; MN=2.39 Nm Shaft height 45 mm, with angle plug; absolute encoder 20-bits (12-bit multi-turn) plain shaft, Tolerance N without holding brake Degree of protection IP65 with sealing ring compatible with the converters SINAMICS V70 & V90",1148,"ΤΕΜ",1,"MC",1,"1FL60441AF612LG1"]
["1FL6090-1AC61-2AH1","SIMOTICS S-1FL6-1FL6 Operating voltage 3AC 400 V Pn=2.5 kW; Nn=2000 rpm M0=15 Nm; MN=11.9 Nm Shaft height 90 mm, with angle plug; incremental encoder 2500 incr./rev. plain shaft, Tolerance N with holding brake Degree of protection IP65 with sealing ring compatible with the converters SINAMICS V70 & V90",1721,"ΤΕΜ",1,"MC",1,"1FL60901AC612AH1"]
["1FN3004-0TK02-1AE0","SIMOTICS L Cooling profile for secondary section 600 series Hollow aluminum profile; per secondary section track 3 units required Length in number of secondary parts, with adapter nipple for (combi-) end piece Price per secondary section segment Number=0+4",124,"ΤΕΜ",1,"MC",1,"1FN30040TK021AE0"]
["1FN3100-1PK10-0AA0","SIMOTICS L precision cooler for primary section 1FN3100-1N... Component 3-phase synchronous motor",417,"ΤΕΜ",1,"MC",1,"1FN31001PK100AA0"]
["1FN3150-1NC20-0BA3","SIMOTICS L primary section; Component 3-phase synchronous motor; Continuous load model; Cover prepared for 2 metric threaded joints; Connection of power and signal separated; with FN=455N; Fmax=770N; Vmax FN=234m/min; Vmax Fmax=129 m/min; In=4.5A; Imax=9.4A with PTC120 and Temperature sensor Pt1000",2331,"ΤΕΜ",1,"MC",1,"1FN31501NC200BA3"]
["1FN3450-3WB50-0BA3","SIMOTICS L primary section; Component 3-phase synchronous motor; Peak load version; Cover prepared for 2 metric threaded joints; Connection of power and signal separated; FN=2895N; Fmax=7760N; Vmax FN=217 m/min; Vmax Fmax=90 m/min; In=22.8 A; Imax=67.3A with PTC120 and Temperature sensor Pt1000",3907,"ΤΕΜ",1,"MC",1,"1FN34503WB500BA3"]
["1FN3600-2WA50-0BA3","SIMOTICS L primary section; Component 3-phase synchronous motor; Peak load version; Cover prepared for 2 metric threaded joints; Connection of power and signal separated; FN=2610N; Fmax=6900N; Vmax FN=120m/min; Vmax Fmax=36m/min; In=12.4A; Imax=36A with PTC120 and Temperature sensor Pt1000",3597,"ΤΕΜ",1,"MC",1,"1FN36002WA500BA3"]
["1FN3900-4WC00-0AA3","SIMOTICS L primary section; Component 3-phase synchronous motor; Peak load version; Connection of power and signal in one cable; Cover prepared for a cable gland; FN=8100N; Fmax=20700N; Vmax FN=253m/min; Vmax Fmax=115m/min; In=73.5A; Imax=206.5A with PTC120 and Temperature sensor Pt1000",5899,"ΤΕΜ",1,"MC",1,"1FN39004WC000AA3"]
["1FT7034-5AK70-1CB0","SIMOTICS S Synchronous motor 1FT7, M0=2Nm (100K) NN=6000rpm, PN=0.88kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5160,"ΤΕΜ",1,"MC",1,"1FT70345AK701CB0"]
["1FT7034-5AK71-1DK4","SIMOTICS S Synchronous motor 1FT7, M0=2Nm (100K) NN=6000rpm, PN=0.88kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",4118,"ΤΕΜ",1,"MC",1,"1FT70345AK711DK4"]
["1FT7036-5AK71-1FA0","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=6000rpm, PN=1.07kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",4683,"ΤΕΜ",1,"MC",1,"1FT70365AK711FA0"]
["1FT7042-5AF70-1FB3","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=3000rpm, PN=0.85kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",5696,"ΤΕΜ",1,"MC",1,"1FT70425AF701FB3"]
["1FT7042-5AF71-1FA0","SIMOTICS S Synchronous motor 1FT7, M0=3Nm (100K) NN=3000rpm, PN=0.85kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",4732,"ΤΕΜ",1,"MC",1,"1FT70425AF711FA0"]
["1FT7044-1AF71-1BG1","SIMOTICS S Synchronous motor 1FT7, M0=5Nm (100K) NN=3000rpm, PN=1.35kW naturally cooled; Power connector rotatable; Vibration severity A Degree of protection IP65 Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACCURACY TOLERANCE N",3272,"ΤΕΜ",1,"MC",1,"1FT70441AF711BG1"]
["1FT7044-5AF70-1DH0","SIMOTICS S Synchronous motor 1FT7, M0=5Nm (100K) NN=3000rpm, PN=1.35kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5057,"ΤΕΜ",1,"MC",1,"1FT70445AF701DH0"]
["1FT7044-5AF71-1DH0","SIMOTICS S Synchronous motor 1FT7, M0=5Nm (100K) NN=3000rpm, PN=1.35kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5057,"ΤΕΜ",1,"MC",1,"1FT70445AF711DH0"]
["1FT7044-5AK71-1CH2","SIMOTICS S Synchronous motor 1FT7, M0=5Nm (100K) NN=6000rpm, PN=1.41kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",6044,"ΤΕΜ",1,"MC",1,"1FT70445AK711CH2"]
["1FT7046-5AF70-1FH1","SIMOTICS S Synchronous motor 1FT7, M0=7Nm (100K) NN=3000rpm, PN=1.76kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6395,"ΤΕΜ",1,"MC",1,"1FT70465AF701FH1"]
["1FT7046-5AF71-1DH0","SIMOTICS S Synchronous motor 1FT7, M0=7Nm (100K) NN=3000rpm, PN=1.76kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5407,"ΤΕΜ",1,"MC",1,"1FT70465AF711DH0"]
["1FT7046-5AH71-1DH1","SIMOTICS S Synchronous motor 1FT7, M0=7Nm (100K) NN=4500rpm, PN=1.32kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",5517,"ΤΕΜ",1,"MC",1,"1FT70465AH711DH1"]
["1FT7062-5AF71-1FG1","SIMOTICS S Synchronous motor 1FT7, M0=6Nm (100K) NN=3000rpm, PN=1.70kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE Absolute encoder 22-bit Multiturn with DRIVE-CLiQ interface (encoder AM22DQ) Rotatable connector PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",5197,"ΤΕΜ",1,"MC",1,"1FT70625AF711FG1"]
["1FT7062-5AK71-1BG2","SIMOTICS S Synchronous motor 1FT7, M0=6Nm (100K) NN=6000rpm, PN=2.13kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",4319,"ΤΕΜ",1,"MC",1,"1FT70625AK711BG2"]
["1FT7062-5WK71-1BG2","SIMOTICS S Synchronous motor 1FT7, M0=10Nm (100K) NN=6000rpm, PN=5.80kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",5060,"ΤΕΜ",1,"MC",1,"1FT70625WK711BG2"]
["1FT7064-5AF71-1CG0","SIMOTICS S Synchronous motor 1FT7, M0=9Nm (100K) NN=3000rpm, PN=2.39kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5482,"ΤΕΜ",1,"MC",1,"1FT70645AF711CG0"]
["1FT7064-5AK70-1BA5","SIMOTICS S Synchronous motor 1FT7, M0=9Nm (100K) NN=6000rpm, PN=2.59kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",4985,"ΤΕΜ",1,"MC",1,"1FT70645AK701BA5"]
["1FT7064-5AK71-1KG2","SIMOTICS S Synchronous motor 1FT7, M0=9Nm (100K) NN=6000rpm, PN=2.59kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) AND M17 CONNECTOR PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",5150,"ΤΕΜ",1,"MC",1,"1FT70645AK711KG2"]
["1FT7065-7WF71-1DK4","SIMOTICS S Synchronous motor 1FT7, M0=19Nm (100K) NN=3000rpm, PN=5.70kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",6318,"ΤΕΜ",1,"MC",1,"1FT70657WF711DK4"]
["1FT7066-5AF71-1DB4","SIMOTICS S Synchronous motor 1FT7, M0=12Nm (100K) NN=3000rpm, PN=2.92kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",6252,"ΤΕΜ",1,"MC",1,"1FT70665AF711DB4"]
["1FT7066-5AH71-1BH2","SIMOTICS S Synchronous motor 1FT7, M0=12Nm (100K) NN=4500rpm, PN=2.55kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",6072,"ΤΕΜ",1,"MC",1,"1FT70665AH711BH2"]
["1FT7066-5WF70-1FH1","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=3000rpm, PN=6.20kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE Absolute encoder 22-bit Multiturn with DRIVE-CLiQ interface (encoder AM22DQ) Rotatable connector PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7687,"ΤΕΜ",1,"MC",1,"1FT70665WF701FH1"]
["1FT7067-7WF70-1CG0","SIMOTICS S Synchronous motor 1FT7, M0=25Nm (100K) NN=3000rpm, PN=7.40kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6983,"ΤΕΜ",1,"MC",1,"1FT70677WF701CG0"]
["1FT7068-5AF71-1FG0","SIMOTICS S Synchronous motor 1FT7, M0=15Nm (100K) NN=3000rpm, PN=3.42kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE Absolute encoder 22-bit Multiturn with DRIVE-CLiQ interface (encoder AM22DQ) Rotatable connector PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6285,"ΤΕΜ",1,"MC",1,"1FT70685AF711FG0"]
["1FT7082-5AC70-1BK5","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=2000rpm, PN=2.39kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",5168,"ΤΕΜ",1,"MC",1,"1FT70825AC701BK5"]
["1FT7082-5AF70-1CG2","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=3000rpm, PN=3.24kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",5684,"ΤΕΜ",1,"MC",1,"1FT70825AF701CG2"]
["1FT7082-5AF71-1LH2","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=3000rpm, PN=3.24kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) AND M17-CONNECTOR PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",7059,"ΤΕΜ",1,"MC",1,"1FT70825AF711LH2"]
["1FT7082-5AH71-1DB1","SIMOTICS S Synchronous motor 1FT7, M0=13Nm (100K) NN=4500rpm, PN=3.77kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",5837,"ΤΕΜ",1,"MC",1,"1FT70825AH711DB1"]
["1FT7084-5AC70-1CG5","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=2000rpm, PN=3.54kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",6726,"ΤΕΜ",1,"MC",1,"1FT70845AC701CG5"]
["1FT7084-5AC71-1LB0","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=2000rpm, PN=3.54kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) AND M17-CONNECTOR SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",7720,"ΤΕΜ",1,"MC",1,"1FT70845AC711LB0"]
["1FT7084-5AF71-1CA2","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=3000rpm, PN=4.55kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",6547,"ΤΕΜ",1,"MC",1,"1FT70845AF711CA2"]
["1FT7084-5AF71-1FH1","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=3000rpm, PN=4.55kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7578,"ΤΕΜ",1,"MC",1,"1FT70845AF711FH1"]
["1FT7084-5AH71-1CB2","SIMOTICS S Synchronous motor 1FT7, M0=20Nm (100K) NN=4500rpm, PN=4.82kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",7577,"ΤΕΜ",1,"MC",1,"1FT70845AH711CB2"]
["1FT7084-5WF71-1FB0","SIMOTICS S Synchronous motor 1FT7, M0=35Nm (100K) NN=3000rpm, PN=11.00kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",8203,"ΤΕΜ",1,"MC",1,"1FT70845WF711FB0"]
["1FT7084-5WH71-1FG2","SIMOTICS S Synchronous motor 1FT7, M0=35Nm (100K) NN=4500rpm, PN=14.60kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",7375,"ΤΕΜ",1,"MC",1,"1FT70845WH711FG2"]
["1FT7086-5AC70-1CH4","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=2000rpm, PN=4.71kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",8781,"ΤΕΜ",1,"MC",1,"1FT70865AC701CH4"]
["1FT7086-5AC71-1FA1","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=2000rpm, PN=4.71kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7664,"ΤΕΜ",1,"MC",1,"1FT70865AC711FA1"]
["1FT7086-5AF70-1FG2","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=3000rpm, PN=5.65kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",7755,"ΤΕΜ",1,"MC",1,"1FT70865AF701FG2"]
["1FT7086-5AF71-1DH1","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=3000rpm, PN=5.65kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7816,"ΤΕΜ",1,"MC",1,"1FT70865AF711DH1"]
["1FT7086-5AH70-1CH0","SIMOTICS S Synchronous motor 1FT7, M0=28Nm (100K) NN=4500rpm, PN=4.71kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",8492,"ΤΕΜ",1,"MC",1,"1FT70865AH701CH0"]
["1FT7086-5WC70-1BH0","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=2000rpm, PN=10.50kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",8350,"ΤΕΜ",1,"MC",1,"1FT70865WC701BH0"]
["1FT7086-5WC71-1CH1","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=2000rpm, PN=10.50kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9338,"ΤΕΜ",1,"MC",1,"1FT70865WC711CH1"]
["1FT7087-7SF70-1CD0","SIMOTICS S Synchronous motor 1FT7, M0=48Nm (100K) NN=3000rpm, PN=10.40kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",9294,"ΤΕΜ",1,"MC",1,"1FT70877SF701CD0"]
["1FT7087-7WH70-1CG1","SIMOTICS S Synchronous motor 1FT7, M0=61Nm (100K) NN=4500rpm, PN=21.70kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9222,"ΤΕΜ",1,"MC",1,"1FT70877WH701CG1"]
["1FT7102-5AB71-1DH0","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=1500rpm, PN=4.08kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",7483,"ΤΕΜ",1,"MC",1,"1FT71025AB711DH0"]
["1FT7102-5AF70-1BA1","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=3000rpm, PN=6.28kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6339,"ΤΕΜ",1,"MC",1,"1FT71025AF701BA1"]
["1FT7102-5AF70-1DG1","SIMOTICS S Synchronous motor 1FT7, M0=30Nm (100K) NN=3000rpm, PN=6.28kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6431,"ΤΕΜ",1,"MC",1,"1FT71025AF701DG1"]
["1FT7102-5WF71-1FH0","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=3000rpm, PN=14.30kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",9097,"ΤΕΜ",1,"MC",1,"1FT71025WF711FH0"]
["1FT7105-5AB70-1DG0","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=1500rpm, PN=6.60kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",8071,"ΤΕΜ",1,"MC",1,"1FT71055AB701DG0"]
["1FT7105-5AB71-1CH2","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=1500rpm, PN=6.60kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",10222,"ΤΕΜ",1,"MC",1,"1FT71055AB711CH2"]
["1FT7105-5AC71-1DK1","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=2000rpm, PN=7.96kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",8365,"ΤΕΜ",1,"MC",1,"1FT71055AC711DK1"]
["1FT7105-5AF70-1FG1","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=3000rpm, PN=8.80kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9060,"ΤΕΜ",1,"MC",1,"1FT71055AF701FG1"]
["1FT7105-5AF71-1CG2","SIMOTICS S Synchronous motor 1FT7, M0=50Nm (100K) NN=3000rpm, PN=8.80kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",9059,"ΤΕΜ",1,"MC",1,"1FT71055AF711CG2"]
["1FT7105-5SC70-1BA1","SIMOTICS S Synchronous motor 1FT7, M0=65Nm (100K) NN=2000rpm, PN=11.70kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",8826,"ΤΕΜ",1,"MC",1,"1FT71055SC701BA1"]
["1FT7105-5SF70-3CG1","SIMOTICS S Synchronous motor 1FT7, M0=65Nm (100K) NN=3000rpm, PN=15.10kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL NON-DRIVE END ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9704,"ΤΕΜ",1,"MC",1,"1FT71055SF703CG1"]
["1FT7105-5WF70-2FA0","SIMOTICS S Synchronous motor 1FT7, M0=90Nm (100K) NN=3000rpm, PN=24.80kW water-cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE LEFT ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",9685,"ΤΕΜ",1,"MC",1,"1FT71055WF702FA0"]
["1FT7105-5WF71-4BG0","SIMOTICS S Synchronous motor 1FT7, M0=90Nm (100K) NN=3000rpm, PN=24.80kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL DRIVE END ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",8715,"ΤΕΜ",1,"MC",1,"1FT71055WF714BG0"]
["1FT7108-5AB71-1DH0","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=1500rpm, PN=9.58kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",11543,"ΤΕΜ",1,"MC",1,"1FT71085AB711DH0"]
["1FT7108-5AC70-1CH3","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=2000rpm, PN=10.50kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",12507,"ΤΕΜ",1,"MC",1,"1FT71085AC701CH3"]
["1FT7108-5AC71-1DH2","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=2000rpm, PN=10.50kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",11745,"ΤΕΜ",1,"MC",1,"1FT71085AC711DH2"]
["1FT7108-5AF70-1BD1","SIMOTICS S Synchronous motor 1FT7, M0=70Nm (100K) NN=3000rpm, PN=6.28kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",10582,"ΤΕΜ",1,"MC",1,"1FT71085AF701BD1"]
["1FT7108-5SC71-1CL1","SIMOTICS S Synchronous motor 1FT7, M0=91Nm (100K) NN=2000rpm, PN=15.30kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",13358,"ΤΕΜ",1,"MC",1,"1FT71085SC711CL1"]
["1FT7108-5SF70-3CG0","SIMOTICS S Synchronous motor 1FT7, M0=91Nm (100K) NN=3000rpm, PN=18.80kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL NON-DRIVE END ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",11903,"ΤΕΜ",1,"MC",1,"1FT71085SF703CG0"]
["1FT7108-5SF75-1MH0","SIMOTICS S Synchronous motor 1FT7, M0=91Nm (100K) NN=3000rpm, PN=18.80kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) recessed flange (more compact), with Pt1000  temperature sensor POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",12662,"ΤΕΜ",1,"MC",1,"1FT71085SF751MH0"]
["1FT7108-5WC74-4NB0","SIMOTICS S Synchronous motor 1FT7, M0=125Nm (100K) NN=2000rpm, PN=26.20kW water-cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with Pt1000 temperature sensor POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL DRIVE END INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",11796,"ΤΕΜ",1,"MC",1,"1FT71085WC744NB0"]
["1FT7132-5AF71-1CG0","SIMOTICS S Synchronous motor 1FT7, M0=90Nm (100K) NN=3000rpm, PN=8.48kW Naturally cooled Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",12353,"ΤΕΜ",1,"MC",1,"1FT71325AF711CG0"]
["1FT7132-5SC74-1NA1","SIMOTICS S Synchronous motor 1FT7, M0=140Nm (100K) NN=2000rpm, PN=26.5 kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible), with Pt1000 temperature sensor POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",12038,"ΤΕΜ",1,"MC",1,"1FT71325SC741NA1"]
["1FT7134-5SC71-1CG1","SIMOTICS S Synchronous motor 1FT7, M0=190 Nm (100K) NN=2000rpm, PN=33.5 kW Forced ventilation Frame size IMB 5 (IM V1, IM V3) Conventional flange (1FT6/1FK7 compatible) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",14677,"ΤΕΜ",1,"MC",1,"1FT71345SC711CG1"]
["1PH8083-1AM10-2BD2","SIMOTICS M Compact asynchronous motor 3000 rpm, 4.1 kW, 13 Nm, 13.6 A, 298 V 3300 rpm, 4.5 kW, 13 Nm, 13.5 A, 327 V 3600 rpm, 4.9 kW, 13 Nm, 14 A, 355 V Forced ventilation; Direction of air flow NDE --> DE; Degree of protection IP55 Without encoder With temperature sensor Pt1000 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE D-END SIGNAL CONNECTION LEFT",3781,"ΤΕΜ",1,"MC",1,"1PH80831AM102BD2"]
["1PH8083-1DG02-0GA1","SIMOTICS M Compact induction motor 2000rpm, 3.7kW 18Nm, 11.6A, 293V 2300rpm, 4.1kW 17Nm, 11.3A, 332V 2650rpm, 4.6 kW 17Nm, 11.2A, 376V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5123,"ΤΕΜ",1,"MC",1,"1PH80831DG020GA1"]
["1PH8083-1DM02-0DH1","SIMOTICS M Compact induction motor 3000rpm, 4.1kW 13Nm, 13.6A, 293V 3300RPM, 4.5kW 13Nm, 13.5A, 332V 3600RPM 4.9kW 13Nm, 14A, 376V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE SR/A; SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY D-END SIGNAL CONNECTION LEFT",5760,"ΤΕΜ",1,"MC",1,"1PH80831DM020DH1"]
["1PH8083-1SF00-1LA1","SIMOTICS M Compact induction motor 1500rpm, 2.8kW 18Nm, 7.5A, 346V 1750rpm, 3.3kW 18Nm, 7.5A, 398V 2000rpm, 3.7kW 18Nm, 7.6A, 447V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 19-bit Without commutation position (encoder IN19DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7468,"ΤΕΜ",1,"MC",1,"1PH80831SF001LA1"]
["1PH8087-1DF02-0CC1","SIMOTICS M Compact induction motor 1500rpm, 3.7kW, 24Nm, 10A, 336V 1750rpm, 4.3kW, 23Nm, 10A, 396V 2000rpm, 4.9kW, 23Nm, 10A, 435V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5872,"ΤΕΜ",1,"MC",1,"1PH80871DF020CC1"]
["1PH8087-1DN12-1DF1","SIMOTICS M Compact induction motor 4500rpm, 5.8kW 12Nm, 19.5A, 315V 5000rpm, 6.5kW 12Nm, 19.5A, 335V 5500rpm, 6.9kW 12Nm, 19A, 370V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE SR/A; SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5953,"ΤΕΜ",1,"MC",1,"1PH80871DN121DF1"]
["1PH8087-1UF02-0LA1","SIMOTICS M Compact induction motor 1500rpm, 3.7kW, 24Nm, 10A, 336V 1750rpm, 4.3kW, 23Nm, 10A, 396V 2000rpm, 4.9kW, 23Nm, 10A, 435V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 20-bit Without commutation position (encoder IN20DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6519,"ΤΕΜ",1,"MC",1,"1PH80871UF020LA1"]
["1PH8101-1UF12-2LA1","SIMOTICS M Compact induction motor 1500rpm, 3.7kW 24Nm, 12.5A, 265V 1750rpm, 4.3kW 23Nm, 12.5A, 304V 2000rpm, 4.7kW 22Nm, 12.5A, 343V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 20-bit Without commutation position (encoder IN20DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6612,"ΤΕΜ",1,"MC",1,"1PH81011UF122LA1"]
["1PH8103-1DF00-2FA1","SIMOTICS M Compact induction motor 1500rpm, 5.5 kW 35Nm, 13.1A, 342V 1750rpm, 6.3kW 34Nm, 13.5A, 412V 2000rpm, 7.0 kW 33Nm, 12.7A, 460 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: INCREASED RADIAL FORCES, VIBRATION SEVERITY GRADE: R/A, SHAFT+FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5773,"ΤΕΜ",1,"MC",1,"1PH81031DF002FA1"]
["1PH8103-1DF12-1BA1","SIMOTICS M Compact induction motor 1500rpm, 5.5 kW 35Nm, 13.1A, 368V 1750rpm, 6.3kW 34Nm, 13.5A, 412V 2000rpm, 7 kW 33Nm, 12.7A, 460 V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5903,"ΤΕΜ",1,"MC",1,"1PH81031DF121BA1"]
["1PH8103-1DG22-0BA1","SIMOTICS M Compact induction motor 2000rpm, 9.5kW 45Nm, 23.8A, 343V 2300rpm, 10.9kW 45Nm, 23.8A, 390V 2650rpm, 12.5kW 45Nm, 23.5A, 454V water cooling Degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6383,"ΤΕΜ",1,"MC",1,"1PH81031DG220BA1"]
["1PH8103-1FF13-0CA1","SIMOTICS M Compact induction motor 1500rpm, 5.5 kW 35Nm, 13.1A, 368V 1750rpm, 6.3kW 34Nm, 13.5A, 412V 2000rpm, 7 kW 33Nm, 12.7A, 460 V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7460,"ΤΕΜ",1,"MC",1,"1PH81031FF130CA1"]
["1PH8103-1SM00-0LF1","SIMOTICS M Compact induction motor 3000rpm, 8.4kW 27Nm, 25.7A, 297V 3300RPM, 9.3kW 27Nm, 25.7A, 326V 3600RPM 10 kW 27Nm, 25.4A, 355V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 19-bit Without commutation position (encoder IN19DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",7828,"ΤΕΜ",1,"MC",1,"1PH81031SM000LF1"]
["1PH8105-1DF00-0BA1","SIMOTICS M Compact induction motor 1500rpm, 7.0 kW 45Nm, 17.5A, 348V 1750rpm, 8.0kW 44Nm, 17.5A, 400 V 2000rpm, 9.0kW 43Nm, 17.0A, 453V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5898,"ΤΕΜ",1,"MC",1,"1PH81051DF000BA1"]
["1PH8105-1DF12-1LC1","SIMOTICS M Compact induction motor 1500rpm, 7kW, 45Nm, 17.5A, 348V 1750rpm, 8kW, 44Nm, 17.5A, 400 V 2000rpm, 9kW, 43Nm, 17A, 453V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",6718,"ΤΕΜ",1,"MC",1,"1PH81051DF121LC1"]
["1PH8105-1SF12-3LA1","SIMOTICS M Compact induction motor 1500rpm, 7kW, 45Nm, 17.5A, 348V 1750rpm, 8kW, 44Nm, 17.5A, 400 V 2000rpm, 9kW, 43Nm, 17A, 453V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 19-bit Without commutation position (encoder IN19DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN HOLLOW-SHAFT BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",10033,"ΤΕΜ",1,"MC",1,"1PH81051SF123LA1"]
["1PH8107-1DD02-1HA1","SIMOTICS M Compact induction motor 1000rpm, 6.3kW 60Nm, 17.5A, 307V 1150rpm, 7.2kW 60Nm, 17.5A, 348V 1350rpm, 8.0kW 57Nm, 17A, 400 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6184,"ΤΕΜ",1,"MC",1,"1PH81071DD021HA1"]
["1PH8107-1DF03-1BB1","SIMOTICS M Compact induction motor 1500rpm, 9.0kW 57Nm, 23.5A, 330V 1750rpm, 10.0kW 55Nm, 22A, 380 V 2000rpm, 11 kW 53Nm, 21.5A, 428V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",6564,"ΤΕΜ",1,"MC",1,"1PH81071DF031BB1"]
["1PH8107-1DF23-1BA1","SIMOTICS M Compact induction motor 1500rpm, 14kW 89Nm, 43.4A, 277V 1750rpm, 15.5kW 85Nm, 42A, 314V 2000rpm, 18kW 86Nm, 42.6A, 363V water cooling Degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7412,"ΤΕΜ",1,"MC",1,"1PH81071DF231BA1"]
["1PH8107-1DG10-2GA1","SIMOTICS M Compact induction motor 2000rpm, 10.5kW 50Nm, 26 A, 355V 2300rpm, 12.5kW 50Nm, 26 A, 406V 2650rpm, 13kW 47Nm, 24A, 460 V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5732,"ΤΕΜ",1,"MC",1,"1PH81071DG102GA1"]
["1PH8107-1DS02-0LA1","SIMOTICS M Compact induction motor Y2000RPM, 11 kW 53Nm, 26.7A, 368V D5000RPM, 11 kW 21Nm, 28A, 410V Y1500RPM, 8.5kW 54Nm, 27A, 275V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6882,"ΤΕΜ",1,"MC",1,"1PH81071DS020LA1"]
["1PH8107-1HF10-2HA2","SIMOTICS M Compact asynchronous motor 1500 rpm, 9 kW, 57 Nm, 23.5 A, 330 V 1750 rpm, 10 kW, 55 Nm, 22 A, 380 V 2000 rpm, 11 kW, 53 Nm, 21.5 A, 428 V Forced ventilation; Direction of air flow NDE --> DE; Degree of protection IP55 Incremental encoder HTL 1024 S/R (encoder HTL1024S/R) With temperature sensor Pt1000 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4777,"ΤΕΜ",1,"MC",1,"1PH81071HF102HA2"]
["1PH8107-1UG02-2LA1","SIMOTICS M Compact induction motor 2000rpm, 10.5kW 50Nm, 26 A, 355V 2300rpm, 12kW 50Nm, 26 A, 406V 2650rpm, 13kW 47Nm, 24A, 460 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 20-bit Without commutation position (encoder IN20DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7121,"ΤΕΜ",1,"MC",1,"1PH81071UG022LA1"]
["1PH8131-1DF00-2CA1","SIMOTICS M Compact induction motor 1500rpm, 11kW, 70 Nm, 24A, 360V 1750rpm, 13kW, 71Nm, 24A, 416V 2000rpm, 15 kW, 72Nm, 24A, 460 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6472,"ΤΕΜ",1,"MC",1,"1PH81311DF002CA1"]
["1PH8131-1DF12-2BB1","SIMOTICS M Compact induction motor 1500rpm, 11kW, 70 Nm, 24A, 360V 1750rpm, 13kW, 71Nm, 24A, 416V 2000rpm, 15 kW, 72Nm, 24A, 460 V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",6522,"ΤΕΜ",1,"MC",1,"1PH81311DF122BB1"]
["1PH8131-2DL00-1BA1","SIMOTICS M Compact synchronous motor 2500rpm, 25kW 96Nm, 44A, 371V 2800rpm, 27.7kW 95Nm, 44A, 415 V 3000rpm, 29.5kW 94Nm, 43A, 449V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",12437,"ΤΕΜ",1,"MC",1,"1PH81312DL001BA1"]
["1PH8131-2FL00-1QE1","SIMOTICS M Compact synchronous motor 2500rpm, 25kW 96Nm, 44A, 371V 2800rpm, 27.7kW 95Nm, 44A, 415 V 3000rpm, 29.5kW 94Nm, 43A, 449V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: ADVANCED LIFETIME VIBRATION SEVERITY S/A SHAFT A. FLANGE ACCURACY GR. R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",13990,"ΤΕΜ",1,"MC",1,"1PH81312FL001QE1"]
["1PH8133-1DD10-1BE1","SIMOTICS M Compact induction motor 1000rpm, 12kW 115Nm, 30 A, 319V 1150rpm, 13.5kW 112Nm, 29A, 361V 1350rpm, 15 kW 106Nm, 28A, 417V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6391,"ΤΕΜ",1,"MC",1,"1PH81331DD101BE1"]
["1PH8133-1DD13-0BA1","SIMOTICS M Compact induction motor 1000rpm, 12kW 115Nm, 30 A, 319V 1150rpm, 13.5kW 112Nm, 29A, 361V 1350rpm, 15 kW 106Nm, 28A, 417V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7018,"ΤΕΜ",1,"MC",1,"1PH81331DD130BA1"]
["1PH8133-1DF12-2CE1","SIMOTICS M Compact induction motor 1500rpm, 15 kW 96Nm, 34A, 342V 1750rpm, 17.5kW 96Nm, 34A, 392V 2000rpm, 20 kW 96Nm, 34A, 445V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6893,"ΤΕΜ",1,"MC",1,"1PH81331DF122CE1"]
["1PH8133-1DG02-2BH1","SIMOTICS M Compact induction motor 2000rpm, 20 kW 96Nm, 45 A, 350 V 2300rpm, 22.5kW 93Nm, 44A, 400 V 2650rpm, 24 kW 86Nm, 41A, 456V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE D-END SIGNAL CONNECTION LEFT",6667,"ΤΕΜ",1,"MC",1,"1PH81331DG022BH1"]
["1PH8133-1FF13-1BA1","SIMOTICS M Compact induction motor 1500rpm, 15 kW 96Nm, 34A, 342V 1750rpm, 17.5kW 96Nm, 34A, 392V 2000rpm, 20 kW 96Nm, 34A, 445V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8073,"ΤΕΜ",1,"MC",1,"1PH81331FF131BA1"]
["1PH8133-1SF02-0LA1","SIMOTICS M Compact induction motor 1500rpm, 15 kW 96Nm, 34A, 342V 1750rpm, 17.5kW 96Nm, 34A, 392V 2000rpm, 20 kW 96Nm, 34A, 445V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 19-bit Without commutation position (encoder IN19DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8857,"ΤΕΜ",1,"MC",1,"1PH81331SF020LA1"]
["1PH8133-1UG10-1LA1","SIMOTICS M Compact induction motor 2000rpm, 20 kW 96Nm, 45 A, 350 V 2300rpm, 22.5kW 93Nm, 44A, 400 V 2650rpm, 24 kW 86Nm, 41A, 456V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 20-bit Without commutation position (encoder IN20DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7263,"ΤΕΜ",1,"MC",1,"1PH81331UG101LA1"]
["1PH8133-2DL10-2BA1","SIMOTICS M Compact synchronous motor 2500rpm, 31.7kW 121Nm, 55A, 371V 2800rpm, 35.2kW 120Nm, 54A, 415 V 3000rpm, 37.4kW 119Nm, 54A, 449V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",13002,"ΤΕΜ",1,"MC",1,"1PH81332DL102BA1"]
["1PH8135-1DF00-1MG1","SIMOTICS M Compact induction motor 1500rpm, 18.5 kW 118Nm, 43A, 330V 1750rpm, 21.5kW 117Nm, 43A, 383V 2000rpm, 24 kW 115Nm, 43A, 434V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: HIGH PERFORMANCE VIBRATION SEVERITY GRADE SPECIAL/B SHAFT AND FLANGE ACCURACY GR. SPECIAL POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",8288,"ΤΕΜ",1,"MC",1,"1PH81351DF001MG1"]
["1PH8135-1DG23-0BH1","SIMOTICS M Compact induction motor 2000rpm, 29kW, 138Nm, 64A, 348V 2300rpm, 31kW, 129Nm, 61A, 397V 2650rpm, 32 kW, 115Nm, 58A, 448V water cooling Degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE D-END SIGNAL CONNECTION LEFT",8605,"ΤΕΜ",1,"MC",1,"1PH81351DG230BH1"]
["1PH8135-2DF02-2BE1","SIMOTICS M Compact synchronous motor 1500rpm, 23.7kW 151Nm, 43A, 383V 1750rpm, 27.2kW 149Nm, 42A, 415 V 2000rpm, 30.2kW 144Nm, 42A, 449V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",13842,"ΤΕΜ",1,"MC",1,"1PH81352DF022BE1"]
["1PH8135-2DG02-1BE1","SIMOTICS M Compact synchronous motor 2000rpm, 31.4kW 150Nm, 59A, 356V 2300rpm, 35.6kW 148Nm, 59A, 407V 2650rpm, 40.2kW 145Nm, 58A, 449V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",13842,"ΤΕΜ",1,"MC",1,"1PH81352DG021BE1"]
["1PH8137-1DD02-0GA1","SIMOTICS M Compact induction motor 1000rpm, 17kW 162Nm, 43A, 307V 1150rpm, 19.5kW 162Nm, 43A, 350 V 1350rpm, 22 kW 156Nm, 42A, 404V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7141,"ΤΕΜ",1,"MC",1,"1PH81371DD020GA1"]
["1PH8137-1DD10-2LA1","SIMOTICS M Compact induction motor 1000rpm, 17kW 162Nm, 43A, 307V 1150rpm, 19.5kW 162Nm, 43A, 350 V 1350rpm, 22 kW 156Nm, 42A, 404V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7828,"ΤΕΜ",1,"MC",1,"1PH81371DD102LA1"]
["1PH8137-1DF02-2FA1","SIMOTICS M Compact induction motor 1500rpm, 22kW, 140 Nm, 56A, 308V 1750rpm, 25kW, 136Nm, 56A, 352V 2000rpm, 28kW, 134Nm, 55A, 401V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: INCREASED RADIAL FORCES, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7623,"ΤΕΜ",1,"MC",1,"1PH81371DF022FA1"]
["1PH8137-1DG02-2BC1","SIMOTICS M Compact induction motor 2000rpm, 28kW, 134Nm, 60A, 350 V 2300rpm, 29kW, 120Nm, 56A, 400 V 2650rpm, 30 kW, 108Nm, 52A, 460 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",7471,"ΤΕΜ",1,"MC",1,"1PH81371DG022BC1"]
["1PH8137-1ED00-1BA2","SIMOTICS M Compact asynchronous motor 1000 rpm, 17 kW, 162 Nm, 43 A, 307 V 1150 rpm, 19.5 kW, 162 Nm, 43 A, 350 V 1350 rpm, 22 kW, 156 Nm, 42 A, 404 V Forced ventilation; Direction of air flow DE --> NDE; Degree of protection IP55 ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER AM2048S/R) with TEMPERATURE SENSOR Pt1000 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7445,"ΤΕΜ",1,"MC",1,"1PH81371ED001BA2"]
["1PH8137-1FF03-0CA1","SIMOTICS M Compact induction motor 1500rpm, 22kW, 140 Nm, 56A, 308V 1750rpm, 25kW, 136Nm, 56A, 352V 2000rpm, 28kW, 134Nm, 55A, 401V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9103,"ΤΕΜ",1,"MC",1,"1PH81371FF030CA1"]
["1PH8137-1MF02-0LA2","SIMOTICS M Compact asynchronous motor 1500 rpm, 22 kW, 140 Nm, 56 A, 308 V 1750 rpm, 25 kW, 136 Nm, 56 A, 352 V 2000 rpm, 28 kW, 134 Nm, 55 A, 401 V Forced ventilation; Direction of air flow DE --> NDE; Degree of protection IP55 Incremental encoder SIN/COS 1 VPP 2048 S/R with C and D track (encoder IC2048S/R) with temperature sensor Pt1000 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7300,"ΤΕΜ",1,"MC",1,"1PH81371MF020LA2"]
["1PH8137-2DL02-2BA1","SIMOTICS M Compact synchronous motor 2500rpm, 48.4kW 185Nm, 83A, 371V 2800rpm, 53.4kW 182Nm, 82A, 415 V 3000rpm, 56.9kW 181Nm, 81A, 449V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",15047,"ΤΕΜ",1,"MC",1,"1PH81372DL022BA1"]
["1PH8138-1DF20-1BC1","SIMOTICS M Compact induction motor 1500rpm, 30 kW, 191Nm, 80 A, 289V 1750rpm, 33 kW, 180Nm, 77A, 332V 2000rpm, 37kW, 177Nm, 76A, 380 V water cooling Degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",8969,"ΤΕΜ",1,"MC",1,"1PH81381DF201BC1"]
["1PH8138-1HF20-1FB2","SIMOTICS M Compact asynchronous motor 1500 rpm, 30 kW, 191 Nm, 80 A, 289 V 1750 rpm, 33 kW, 180 Nm, 77 A, 332 V 2000 rpm, 37 kW, 177 Nm, 76 A, 380 V Water cooling Degree of protection IP65 Incremental encoder HTL 1024 S/R (encoder HTL1024S/R) With temperature sensor Pt1000 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: INCREASED RADIAL FORCES, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",7941,"ΤΕΜ",1,"MC",1,"1PH81381HF201FB2"]
["1PH8163-1DD03-0BB1","SIMOTICS M Compact induction motor 1000rpm, 22kW, 210Nm, 55A, 300V 1150rpm, 25kW, 208Nm, 55A, 343V 1350rpm, 28kW, 198Nm, 52A, 400 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",9036,"ΤΕΜ",1,"MC",1,"1PH81631DD030BB1"]
["1PH8163-1DF00-2BA1","SIMOTICS M Compact induction motor 1500rpm, 30 kW, 191Nm, 71A, 319V 1750rpm, 34kW, 186Nm, 70A, 366V 2000rpm, 37kW, 177Nm, 68A, 416V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8509,"ΤΕΜ",1,"MC",1,"1PH81631DF002BA1"]
["1PH8163-1DF10-2CA1","SIMOTICS M Compact induction motor 1500rpm, 30 kW, 191Nm, 71A, 319V 1750rpm, 34kW, 186Nm, 70A, 366V 2000rpm, 37kW, 177Nm, 68A, 416V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8735,"ΤΕΜ",1,"MC",1,"1PH81631DF102CA1"]
["1PH8163-1DG00-0MA1","SIMOTICS M Compact induction motor 2000rpm, 36kW, 172Nm, 83A, 324V 2300rpm, 38 kW, 158Nm, 78A, 370V 2650rpm, 40kW, 144Nm, 76A, 390V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: HIGH PERFORMANCE VIBRATION SEVERITY GRADE SPECIAL/B SHAFT AND FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9962,"ΤΕΜ",1,"MC",1,"1PH81631DG000MA1"]
["1PH8163-1UD00-0LA1","SIMOTICS M Compact induction motor 1000rpm, 22kW, 210Nm, 55A, 300V 1150rpm, 25kW, 208Nm, 55A, 343V 1350rpm, 28kW, 198Nm, 52A, 400 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 20-bit Without commutation position (encoder IN20DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9285,"ΤΕΜ",1,"MC",1,"1PH81631UD000LA1"]
["1PH8163-3DB03-2AA1","SIMOTICS M Compact induction motor 400rpm, 9.5kW 227Nm, 30 A, 260V 500rpm, 12kW 229Nm, 30 A, 325V 600rpm, 14.5kW 231Nm, 30 A, 370V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD VIBRATION SEVERITY GRADE A; SHAFT A.FLANGE ACCURACY GR. N TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8813,"ΤΕΜ",1,"MC",1,"1PH81633DB032AA1"]
["1PH8165-1DD02-0DA1","SIMOTICS M Compact induction motor 1000rpm, 28kW, 267Nm, 71A, 292V 1150rpm, 31kW, 257Nm, 69A, 333V 1350rpm, 34kW, 241Nm, 66A, 387V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE SR/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",10009,"ΤΕΜ",1,"MC",1,"1PH81651DD020DA1"]
["1PH8165-1DD13-2BB1","SIMOTICS M Compact induction motor 1000rpm, 28kW, 267Nm, 71A, 292V 1150rpm, 31kW, 257Nm, 69A, 333V 1350rpm, 34kW, 241Nm, 66A, 387V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",9903,"ΤΕΜ",1,"MC",1,"1PH81651DD132BB1"]
["1PH8165-1DF03-2BA1","SIMOTICS M Compact induction motor 1500rpm, 37kW, 236Nm, 78A, 350 V 1750rpm, 41kW, 224Nm, 76A, 400 V 2000rpm, 45kW, 215Nm, 75 A, 440 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9903,"ΤΕΜ",1,"MC",1,"1PH81651DF032BA1"]
["1PH8165-1DG03-0MD1","SIMOTICS M Compact induction motor 2000rpm, 41kW, 196Nm, 88A, 350 V 2300rpm, 44 kW, 183Nm, 85A, 394V 2650rpm, 50 kW, 180Nm, 85A, 440 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: HIGH PERFORMANCE VIBRATION SEVERITY GRADE SPECIAL/B SHAFT AND FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE D-END SIGNAL CONNECTION LEFT",11580,"ΤΕΜ",1,"MC",1,"1PH81651DG030MD1"]
["1PH8165-1FD12-2GB1","SIMOTICS M Compact induction motor 1000rpm, 28kW, 267Nm, 71A, 292V 1150rpm, 31kW, 257Nm, 69A, 333V 1350rpm, 34kW, 241Nm, 66A, 387V forced ventilation; direction of air flow NDE--> DE; Degree of protection IP55 Absolute encoder 22-bit Single-turn and 12-bit multi-turn (encoder AM22DQ) with DRIVE-CLiQ interface DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",10627,"ΤΕΜ",1,"MC",1,"1PH81651FD122GB1"]
["1PH8165-2DL00-1BA1","SIMOTICS M Compact synchronous motor 2500rpm, 84kW 320Nm, 148A, 370V 2800rpm, 87kW 300 Nm, 138A, 410V 3000rpm, 89kW 285Nm, 131A, 440 V forced ventilation; direction of air flow DE--> NDE; Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",17465,"ΤΕΜ",1,"MC",1,"1PH81652DL001BA1"]
["1PH8166-1DF23-2LC1","SIMOTICS M Compact induction motor 1500rpm, 52kW 331Nm, 116A, 332V 1750rpm, 61kW 333Nm, 116A, 381V 2000rpm, 68kW 325Nm, 116A, 426V water cooling Degree of protection IP65 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface Design IM B35 (IM V15, (IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",14428,"ΤΕΜ",1,"MC",1,"1PH81661DF232LC1"]
["1PH8184-1AD03-1LC2","SIMOTICS M Compact asynchronous motor 1000 rpm, 39 kW, 372 Nm, 87 A, 340 V 1150 rpm, 44 kW, 365 Nm, 86 A, 390 V 1350 rpm, 50 kW, 354 Nm, 84 A, 450 V Forced ventilation Direction of air flow DE-->NDE Degree of protection IP55 Without encoder With temperature sensor Pt1000 Design IM B35 with flange A450 (IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE VIBRATION SEVERITY GRADE SR/B SHAFT A. FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION RIGHT",18608,"ΤΕΜ",1,"MC",1,"1PH81841AD031LC2"]
["1PH8186-1DD00-0AC1","SIMOTICS M Compact induction motor 1000rpm, 51kW 487Nm, 112A, 340V 1150rpm, 58kW 482Nm, 112A, 390V 1350rpm, 67kW 474Nm, 112A, 450 V forced ventilation Direction of air flow DE-->NDE Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IMB6, IMB7, IMB8, IMV6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD VIBRATION SEVERITY GRADE A; SHAFT A.FLANGE ACCURACY GR.N TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION RIGHT",15504,"ΤΕΜ",1,"MC",1,"1PH81861DD000AC1"]
["1PH8186-1DD02-1CB1","SIMOTICS M Compact induction motor 1000rpm, 51kW 487Nm, 112A, 340V 1150rpm, 58kW 482Nm, 112A, 390V 1350rpm, 67kW 474Nm, 112A, 450 V forced ventilation Direction of air flow DE-->NDE Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B5 WITH FLANGE A450 (IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD VIBRATION SEVERITY GRADE S/A SHAFT A.FLANGE ACCURACY GR.R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",17921,"ΤΕΜ",1,"MC",1,"1PH81861DD021CB1"]
["1PH8224-1DF10-2BA1","SIMOTICS M Compact induction motor 1500rpm, 95kW, 605Nm, 200 A, 340V 1750rpm, 110 kW, 600Nm, 198A, 395V 2000rpm, 124kW, 592Nm, 196A, 460 V forced ventilation Direction of air flow NDE-->DE Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IMB6, IMB7, IMB8, IMV6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD VIBRATION SEVERITY GRADE R/A; SHAFT A.FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",20107,"ΤΕΜ",1,"MC",1,"1PH82241DF102BA1"]
["1PH8228-1DB10-2FA1","SIMOTICS M Compact induction motor 400rpm, 48kW 1146Nm, 132A, 272V 500rpm, 60kW 1146Nm, 132A, 340V 600rpm, 72kW 1146Nm, 130A, 410V forced ventilation Direction of air flow NDE-->DE Degree of protection IP55 Incremental encoder 22-bit with commutation position (encoder IC22DQ) with DRIVE-CLiQ interface DESIGN IM B3 (IMB6, IMB7, IMB8, IMV6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: GREATER CANTILEVER FORCES; VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",31519,"ΤΕΜ",1,"MC",1,"1PH82281DB102FA1"]
["6AU1810-0FA30-1XE0","SIMOTION ENGINEERING SYSTEM SCOUT EXTENSIONS V3.0 SP1 CAMTOOL UPGRADE FLOATING LICENSE WITH DATA CARRIER CD-ROM MULTILINGUAL (GER/ENG) ONLY FOR SCOUT AND SCOUT Stand-alone AS OF V4.2 SP1",252,"ΤΕΜ",1,"MC",1,"6AU18100FA301XE0"]
["6AU1810-1CA45-0XA0","SIMOTION ENGINEERING SYSTEM SCOUT STANDALONE AND SCOUT TIA V4.5 FULL LICENSE, Data Carrier DVD INCL. STARTER, RUNTIME, TECHN. Documentation, UTILITIES FOR FREE",5077,"ΤΕΜ",1,"MC",1,"6AU18101CA450XA0"]
["6AU1820-3EA20-0AB0","SIMOTION TECHNOLOGY FUNCTION OACAMGEN CAM Generator for Servo Presses SINGLE LICENSE FOR ONE DESTINATION DEVICE",7394,"ΤΕΜ",1,"MC",1,"6AU18203EA200AB0"]
["6FC5263-1PY11-5AG1","solutions for Powertrain HMI LITE for Comfort Panel KTP900F Mobile and TP1200 software version V15.1.1 on DVD single license",684,"ΤΕΜ",1,"MC",1,"6FC52631PY115AG1"]
["6FC5303-1AF10-8AA0","SINUMERIK Push Button Panel MPP 483 IEH Connection Industrial Ethernet with connection for HT8/HT2 with feedrate override",4037,"ΤΕΜ",1,"MC",1,"6FC53031AF108AA0"]
["6FC5303-1AF13-0AP0","SINUMERIK pushbutton panel MPP 483 IE/L-L14 with raised masking frame 244 mm connection Industrial Ethernet without handheld unit connection with feedrate override customer-specific variant based on 6FC5303-1AF10-0AA0",5800,"ΤΕΜ",1,"MC",1,"6FC53031AF130AP0"]
["6FC5370-3AT03-0AA0","SINUMERIK 808D, Extended T PPU 151.3 horizontal with current software version English layout",4086,"ΤΕΜ",1,"MC",1,"6FC53703AT030AA0"]
["6FC5397-1GP40-0CA0","SINUMERIK Documentation SINUMERIK 840D sl Step 7 Toolbox V15 Getting Started Edition 12/17, Italian",56.1,"ΤΕΜ",1,"MC",1,"6FC53971GP400CA0"]
["6FC5397-7EP40-0RA5","SINUMERIK 808D extended Documentation Function Manual Edition 12/18, Simpl. Chin.",50.6,"ΤΕΜ",1,"MC",1,"6FC53977EP400RA5"]
["6FC5398-0AC10-1YA5","SINUMERIK 840D sl SINAMICS/SIMOTICS/SIMATIC USER-/MANUFACTURER-/SERVICE- DOCUMENTATION ON CD-ROM V4.8 SP2, GER/ENG",218,"ΤΕΜ",1,"MC",1,"6FC53980AC101YA5"]
["6FC5398-4BP40-6MA3","SINUMERIK 840D sl/828D Documentation Measuring cycles Programming Manual Edition 12/98, Chin. trad.",145,"ΤΕΜ",1,"MC",1,"6FC53984BP406MA3"]
["6FC5398-6AP41-0AA0","SINUMERIK 840D sl/828D DOCUMENTATION OPERATING MANUAL UNIVERSAL EDITION 08/18, GERMAN",193,"ΤΕΜ",1,"MC",1,"6FC53986AP410AA0"]
["6FC5398-6DP10-0BA6","SINUMERIK 808D, Extended Documentation Diagnostics Manual Edition 07/18 English,",51.1,"ΤΕΜ",1,"MC",1,"6FC53986DP100BA6"]
["6FC5398-8BP40-5KA3","SINUMERIK 828D, SINAMICS S120, ALARMS DOCUMENTATION DIAGNOSTICS MANUAL EDITION 10/15, Portuguese",251,"ΤΕΜ",1,"MC",1,"6FC53988BP405KA3"]
["6FC5398-8CP40-5NA2","SINUMERIK 840D SL/828D DOCUMENTATION OPERATING MANUAL TURNING EDITION 01/15, Polish",227,"ΤΕΜ",1,"MC",1,"6FC53988CP405NA2"]
["6FC5800-0AK80-0YB0","SINUMERIK 808D additional 1 positioning axis/auxiliary spindle software option Delivery of a license",304,"ΤΕΜ",1,"MC",1,"6FC58000AK800YB0"]
["6FC5800-0AM61-0YB0","SINUMERIK 828D/840D sl extended stop and retract ESR (NC-controlled + drive-autonomous from software 4.X) software option delivery of a license",5596,"ΤΕΜ",1,"MC",1,"6FC58000AM610YB0"]
["6FC5800-0AN61-0YB0","SINUMERIK 840D SL SINUMERIK INTEGRATE RUN RUN MYCC /COPA CORRELATED POSITION ACCESS SOFTWARE OPTION DELIVERY OF ONE LICENSE CUSTOMER SPECIFIC RELEASE REQUIRED NOT FOR EXPORT VARIANTS",2253,"ΤΕΜ",1,"MC",1,"6FC58000AN610YB0"]
["6FC5800-0BM15-0YB0","SINUMERIK ONE multi-axis interpolation (>4 interpolating axes) software option requires standard software delivery of an electronic license (PDF) ******************************* email address for delivery is absolutely essential",1811,"ΤΕΜ",1,"MC",1,"6FC58000BM150YB0"]
["6FC5800-0BN10-0YB0","SINUMERIK ONE SINUMERIK Integrate Run MyCC /SUTI servo service programs software option delivery of an electronic license (PDF) ******************************* email address for delivery is absolutely essential",902,"ΤΕΜ",1,"MC",1,"6FC58000BN100YB0"]
["6FC5851-1XC45-4YA8","SINUMERIK 840D sl CNC software 31-3 and SINUMERIK Operate, 6 languages (de, en, fr, sp, it, zh-s) Software 4.8 SP4 on DVD, without license",410,"ΤΕΜ",1,"MC",1,"6FC58511XC454YA8"]
["6FC5851-1XG46-1YA8","SINUMERIK 840D SL CNC-SOFTWARE 31-3 6-LANGUAGES, EN,GER,FR,IT,SP,CH-S SOFTWARE 4.91 ON CF-CARD WITHOUT LICENSE",617,"ΤΕΜ",1,"MC",1,"6FC58511XG461YA8"]
["6FX2001-2DB25","INCREM. ENCODER 6FX2001-2DB25 WITH RS 422 (TTL), 1250 P/R, SYNCHRO-FLANGE SHAFT 6MM OPERATING VOLTAGE: 10 - 30 V UNIVERSAL CABLE OUTLET AXIAL / RADIAL CABLE 1M WITH CONNECTOR",416,"ΤΕΜ",1,"MC",1,"6FX20012DB25"]
["6FX2001-2QB50","INCREM. ENCODER 6FX2001-2QB50 WITH RS 422 (TTL), 1500 P/R, CLAMP FLANGE WELLE 10 MM OPERATING VOLTAGE 10 - 30 V RADIAL FLANGE CONNECTOR",416,"ΤΕΜ",1,"MC",1,"6FX20012QB50"]
["6FX2002-1DC00-1AC2","Signal cable pre-assembled type: 6FX2002-1DC00 (SINAMICS Drive CLiQ) Connector IP20/IP20, without 24 V Length (m)= 0 + 0 + 2 + 0,2",136,"ΤΕΜ",1,"MC",1,"6FX20021DC001AC2"]
["6FX2002-1DC00-1BH0","Signal cable pre-assembled type: 6FX2002-1DC00 (SINAMICS Drive CLiQ) Connector IP20/IP20, without 24 V Length (m)= 0 + 10 + 7 + 0",246,"ΤΕΜ",1,"MC",1,"6FX20021DC001BH0"]
["6FX2002-1DC20-1EE8","Signal cable pre-assembled type: 6FX2002-1DC20 (SINAMICS Drive CLiQ) Connector IP67/IP67, without 24 V Length (m)= 0 + 40 + 4 + 0,8",510,"ΤΕΜ",1,"MC",1,"6FX20021DC201EE8"]
["6FX2003-0SA80","Signal connector 12-pole type: 6FX2003-0SA80 Socket, Male thread Direction of rotation pins for Heidenhain encoder connection Pack=1 unit",57.800000000000004,"ΤΕΜ",1,"MC",1,"6FX20030SA80"]
["6FX5002-2AH00-1AB0","Signal cable pre-assembled (HTL in motor 1-ph.) 4x 2x 0.34+4x 0.5 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm TYPE: 6FX5002-2AH00 LENGTH (M) = 0 + 0 + 1 + 0",91.399999999999991,"ΤΕΜ",1,"MC",1,"6FX50022AH001AB0"]
["6FX5002-2AH11-1DC0","Signal cable pre-assembled type: 6FX5002-2AH11 (basis 6FX5002-2AH00-....) with integrated temperature cores UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm Length (m)= 0 + 30 + 2 + 0",431,"ΤΕΜ",1,"MC",1,"6FX50022AH111DC0"]
["6FX5002-2CA34-1AG0","signal cable, pre-assembled Extension (encoder voltage signal) 3x 2x 0.14+4x 0.14+2x0.5+4x 0.22 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.9 mm TYPE: 6FX5002-2CA34 LENGTH (M) = 0 + 0 + 6 + 0",212,"ΤΕΜ",1,"MC",1,"6FX50022CA341AG0"]
["6FX5002-2CC11-1AF0","Signal cable pre-assembled (SSI absolute encoder SSI6FX2001-5) 4x 2x 0.34+4x 0.5 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm TYPE: 6FX5002-2CC11 LENGTH (M) = 0 + 0 + 5 + 0",153,"ΤΕΜ",1,"MC",1,"6FX50022CC111AF0"]
["6FX5002-2CG00-1CA0","Signal cable pre-assembled (810D/611D to incremental encoder) 4x 2x 0.34+4x 0.5 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm TYPE: 6FX5002-2CG00 LENGTH (M) = 0 + 20 + 0 + 0",229,"ΤΕΜ",1,"MC",1,"6FX50022CG001CA0"]
["6FX5002-2DC00-1AC6","Signal cable pre-assembled type: 6FX5002-2DC00 (SINAMICS Drive CLiQ) connector IP20/IP20, with 24 V MOTION-CONNECT 500 Length (m)= 0 + 0 + 2 + 0,6",124,"ΤΕΜ",1,"MC",1,"6FX50022DC001AC6"]
["6FX5002-2DC10-1AG1","Signal cable pre-assembled type: 6FX5002-2DC10 (SINAMICS Drive CLiQ) connector IP20/IP67, with 24 V MOTION-CONNECT 500 Length (m)= 0 + 0 + 6 + 0,1",172,"ΤΕΜ",1,"MC",1,"6FX50022DC101AG1"]
["6FX5002-2DC20-1AB0","Signal cable pre-assembled type: 6FX5002-2DC20 (SINAMICS Drive CLiQ) connector IP67/IP67, with 24 V MOTION-CONNECT 500 Length (m)= 0 + 0 + 1 + 0",146,"ΤΕΜ",1,"MC",1,"6FX50022DC201AB0"]
["6FX5002-2DC30-1BK0","DRIVE-CLiQ cable type: 6FX5002-2DC30 Pre-assembled for direct measuring systems with 24 V Connector RJ45, IP20 and Mating connector M12, IP67 MOTION-CONNECT 500 UL/CSA, DESINA Dmax=7.1 mm Length (m)=19",276,"ΤΕΜ",1,"MC",1,"6FX50022DC301BK0"]
["6FX5002-2DC36-1EF0","Signal cable pre-assembled Type: 6FX5002-2DC36 DRIVE-CLiQ with 24 V M12 female/ RJ45 IP67, MOTION-CONNECT 500 Dmax=7.1 mm length (m)=45",509,"ΤΕΜ",1,"MC",1,"6FX50022DC361EF0"]
["6FX5002-2DC46-1GF0","Signal cable pre-assembled Type: 6FX5002-2DC46 DRIVE-CLiQ with 24 V M12 female/ M17 male speed-connect-ready MOTION-CONNECT 500 Dmax=7.1 mm length (m)=65",761,"ΤΕΜ",1,"MC",1,"6FX50022DC461GF0"]
["6FX5002-5CA68-1AC0","power cable, pre-assembled, Extension 4x 10 C, Connector Sz. 1.5 (1FT/1FK to 611/810D/SIMOVERT) UL/CSA DESINA MOTION-CONNECT 500 Dmax=20.0 mm TYPE: 6FX5002-5CA68 LENGTH (M) = 0 + 0 + 2 + 0",399,"ΤΕΜ",1,"MC",1,"6FX50025CA681AC0"]
["6FX5002-5CF10-1AD0","power cable type: 6FX5002-5CF10 pre-assembled 4x 1.5 C, SPEED-CONNECT Sz. 1 for SINAMICS S120 Combi MOTION-CONNECT 500 UL/CSA, DESINA Dmax=8.4 mm Length (m)= 0 + 0 + 3 + 0",140,"ΤΕΜ",1,"MC",1,"6FX50025CF101AD0"]
["6FX5002-5CG10-1CJ0","Power cable pre-assembled 4x 1.5 C SPEED-CONNECT connector Sz. 1 (SINAMICS AC Drive) UL/CSA DESINA MOTION-CONNECT 500 Dmax=8.4 mm TYPE: 6FX5002-5CG10 LENGTH (M) = + 0 + 20 + 8 + 0",272,"ΤΕΜ",1,"MC",1,"6FX50025CG101CJ0"]
["6FX5002-5CG22-1DG0","Power cable pre-assembled 4x 1.5 C Speed connect connector Sz. 1.5 (SINAMICS AC Drive) UL/CSA DESINA MOTION-CONNECT 500 Dmax=8.4 mm TYPE: 6FX5002-5CG22 LENGTH (M) = + 0 + 30 + 6 + 0",497,"ΤΕΜ",1,"MC",1,"6FX50025CG221DG0"]
["6FX5002-5CN06-1AH5","Power cable pre-assembled TYPE 6FX5002-5CN06 4X1,5 C, SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX=8.4 MM LENGTH (M) = + 0 + 0 + 7 + 0.5",245,"ΤΕΜ",1,"MC",1,"6FX50025CN061AH5"]
["6FX5002-5CN27-1BA0","Power cable pre-assembled TYPE 6FX5002-5CN27 4X1,5C, SPEED-CONNECT SIZE 0.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX=8.4 MM LENGTH (M) = + 0 + 10 + 0 + 0",256,"ΤΕΜ",1,"MC",1,"6FX50025CN271BA0"]
["6FX5002-5CS06-1BG0","Power cable pre-assembled TYPE 6FX5002-5CS06 4X1,5 C, CONN. FULL THREAD S. 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX=8.4 MM LENGTH (M) = + 0 + 10 + 6 + 0",279,"ΤΕΜ",1,"MC",1,"6FX50025CS061BG0"]
["6FX5002-5CS46-1AF0","Power cable pre-assembled TYPE 6FX5002-5CS46 4X4 C CONNECTOR FULL THREAD SIZE 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX=11.4 MM LENGTH (M) = + 0 + 0 + 5 + 0",313,"ΤΕΜ",1,"MC",1,"6FX50025CS461AF0"]
["6FX5002-5CS64-1BA0","Power cable pre-assembled type: 6FX5002-5CS64 (1FT/1FK/1PH for SINAMICS) 4x 10 C, Connector Sz. 1.5/ Ring cable lug UL/CSA, DESINA MOTION-CONNECT 500 Dmax=20 mm; Length (m)= 0 + 10 + 0 + 0",429,"ΤΕΜ",1,"MC",1,"6FX50025CS641BA0"]
["6FX5002-5DG01-1AA3","Power cable pre-assembled type: 6FX5002-5DG01 4x 1.5+(2x1.5) C, Connector Sz. 1 (SINAMICS AC Drive) UL/CSA, DESINA MOTION-CONNECT 500 Dmax=10.8 mm 0 + 0 + 0 + 0,3",164,"ΤΕΜ",1,"MC",1,"6FX50025DG011AA3"]
["6FX5002-5DG11-1AC0","Power cable pre-assembled type: 6FX5002-5DG11 4x 2.5+(2x1.5) C, Connector Sz. 1 (SINAMICS AC Drive) UL/CSA, DESINA MOTION-CONNECT 500 Dmax=12.4 mm 0 + 0 + 2 + 0",177,"ΤΕΜ",1,"MC",1,"6FX50025DG111AC0"]
["6FX5002-5DN05-1AD0","power cable, pre-assembled, Extension 4x 1.5+(2x1.5) C SPEED-CONNECT connector Sz. 1 (SIMODRIVE) UL/CSA DESINA MOTION-CONNECT 500 Dmax=13.1 mm TYPE: 6FX5002-5DN05 LENGTH (M) = + 0 + 0 + 3 + 0",285,"ΤΕΜ",1,"MC",1,"6FX50025DN051AD0"]
["6FX5002-5DN27-1DF0","Power cable pre-assembled TYPE 6FX5002-5DN27 4X1.5, (2X1.5)C C CONNECTOR SPEED-CONNECT SIZE 0.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX = 10.8 MM LENGTH (M) = + 0 + 30 + 5 + 0",462,"ΤΕΜ",1,"MC",1,"6FX50025DN271DF0"]
["6FX5002-5DN46-1CA0","Power cable pre-assembled TYPE 6FX5002-5DN46 4X4, (2X1.5)C C CONNECTOR SPEED-CONNECT S. 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 500 UL/CSA, DESINA DMAX=14 MM LENGTH (M) = + 0 + 20 + 0 + 0",516,"ΤΕΜ",1,"MC",1,"6FX50025DN461CA0"]
["6FX5002-5ME05-1BA0","Power cable pre-assembled type: 6FX5002-5ME05 Extension Basis 5DA05 with connector Sz. 0.5; UL/CSA, DESINA MOTION-CONNECT 500 Length (m)= 0 + 10 + 0 + 0",285,"ΤΕΜ",1,"MC",1,"6FX50025ME051BA0"]
["6FX5002-8QN11-1BF0","Single cable connection prefabricated 4G1.5+1Q0,2STC+1P1.5C-C SPEED-CONNECT connector M23 Cores with end sleeve Data cable with IX connector UL/CSA DESINA MOTION-CONNECT 500 Dmax.=12.3 MM Length(M)= 0 + 10 + 5 + 0",474,"ΤΕΜ",1,"MC",1,"6FX50028QN111BF0"]
["6FX5008-1BB05-1EJ0","Power cable sold by the meter type: 6FX5008-1BB05 4x 95 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=51.7 mm, Length (m)= 0 + 40 + 8 + 0",8784,"ΤΕΜ",1,"MC",1,"6FX50081BB051EJ0"]
["6FX5008-1BB41-1CJ0","Power cable sold by the meter type: 6FX5008-1BB41 4x 6.0 C UL/CSA, DESINA MOTION-CONNECT 500 Type of delivery: to 69 m ring from 70 m drum Dmax=13.6 mm, Length (m)= 0 + 20 + 8 + 0",445,"ΤΕΜ",1,"MC",1,"6FX50081BB411CJ0"]
["6FX5008-1BB50-1AE0","Power cable sold by the meter type: 6FX5008-1BB50 4x 50 C UL/CSA, DESINA MOTION-CONNECT 500 Type of delivery: to 9 m ring from 10 m drum Dmax=38.0 mm, Length (m)= 0 + 0 + 4 + 0",363,"ΤΕΜ",1,"MC",1,"6FX50081BB501AE0"]
["6FX5008-1BB70-1EF0","Power cable sold by the meter type: 6FX5008-1BB70 4x 70 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=42.6 mm, Length (m)= 0 + 40 + 5 + 0",6854,"ΤΕΜ",1,"MC",1,"6FX50081BB701EF0"]
["6FX5012-2CH00-1FA0","Signal cable pre-assembled (810D/611D to encoder EnDat) 3x 2x 0.14+4x 0.14+2x0.5 C UL/CSA, DESINA MOTION-CONNECT 500 Dmax=9.3 mm TYPE: 6FX5012-2CH00 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = 0 + 50 + 0 + 0",488,"ΤΕΜ",1,"MC",1,"6FX50122CH001FA0"]
["6FX7002-5EA48-1AJ0","power cable, pre-assembled Extension type: 6FX7002-5EA48 4x 4+(4x 0.5) C, Connector Sz. 1.5 (1FN to 611) trailable UL/CSA DESINA MOTION-CONNECT 700 Dmax=16.6 mm, Length (m)= 0 + 0 + 8 + 0",630,"ΤΕΜ",1,"MC",1,"6FX70025EA481AJ0"]
["6FX7002-5LM42-1AC0","Power cable pre-assembled type: 6FX7002-5LM42 4x 2.5 C M20/1FN3 screw connection Connector full thread Sz. 1 on the converter side for SIMODRIVE/MASTERDRIVES MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=11 mm Length (m)= 0 + 0 + 2 + 0",266,"ΤΕΜ",1,"MC",1,"6FX70025LM421AC0"]
["6FX7008-1BC11-1AH0","Power cable sold by the meter type: 6FX7008-1BC11 4x 1.5+4x 0.5 C for linear motors trailable UL/CSA DESINA MOTION-CONNECT 700 Type of delivery: Ring Dmax=14.0 mm, Length (m)= 0 + 0 + 7 + 0",216,"ΤΕΜ",1,"MC",1,"6FX70081BC111AH0"]
["6FX8002-2AD04-1AF5","Signal cable pre-assembled for absolute value encoder SSI and EnDat 5V DC, also extension for base 6FX8002-2AD00-XXXX 3x (2x0.14) C+4x 0.14+2x0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.2 mm TYPE: 6FX8002-2AD04 LENGTH (M) = 0 + 0 + 5 + 0,5",251,"ΤΕΜ",1,"MC",1,"6FX80022AD041AF5"]
["6FX8002-2CA11-1AF2","Signal cable pre-assembled for incremental encoder sin/cos 1 Vpp 6FX2001-3 4x (2x0.34)+4x 0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.3 mm Length (m)= TYPE: 6FX8002-2CA11 LENGTH (M) = + 0 + 0 + 5 + 0,2",175,"ΤΕΜ",1,"MC",1,"6FX80022CA111AF2"]
["6FX8002-2CA31-1AF0","Signal cable pre-assembled for incr. encoder with C/D tracks integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2CA31 LENGTH (M) = + 0 + 0 + 5 + 0",217,"ΤΕΜ",1,"MC",1,"6FX80022CA311AF0"]
["6FX8002-2CA31-1CH0","Signal cable pre-assembled for incr. encoder with C/D tracks integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2CA31 LENGTH (M) = + 0 + 20 + 7 + 0",474,"ΤΕΜ",1,"MC",1,"6FX80022CA311CH0"]
["6FX8002-2CA80-1BE0","Signal cable pre-assembled type: 6FX8002-2CA80 for incremental encoder SIN/COS 1 VPP without C and D track 3x (2x0.14) C+4x 0.14+2x0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.2 mm Length (m)= 0 + 10 + 4 + 0",327,"ΤΕΜ",1,"MC",1,"6FX80022CA801BE0"]
["6FX8002-2CE31-1BF0","Signal cable pre-assembled type: 6FX8002-2CE31 Customer-specific Length (m)= 0 + 10 + 5 + 0",422,"ΤΕΜ",1,"MC",1,"6FX80022CE311BF0"]
["6FX8002-2CF02-1EA0","Signal cable pre-assembled For resolvers 3x (2x0.14) C+4x 0.14+2x0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.2 mm Length (m)= TYPE: 6FX8002-2CF02 LENGTH (M) = 0 + 40 + 0 + 0",620,"ΤΕΜ",1,"MC",1,"6FX80022CF021EA0"]
["6FX8002-2CG00-1CF0","Signal cable pre-assembled for incremental encoder SIN/COS 1VPP, 6FX2001-3 4x (2x0.34)+4x 0.5 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.3 mm Length (m)= TYPE: 6FX8002-2CG00 LENGTH (M) = 0 + 20 + 5 + 0",328,"ΤΕΜ",1,"MC",1,"6FX80022CG001CF0"]
["6FX8002-2CP00-1AD5","Signal cable pre-assembled type: 6FX8002-2CP00 for handwheel 840D on COM board 4x (2x0.18) C MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=6.7 mm Length (m)= 0 + 0 + 3 + 0,5",121,"ΤΕΜ",1,"MC",1,"6FX80022CP001AD5"]
["6FX8002-2DC10-1AF2","signal cable, pre-assembled type: 6FX8002-2DC10 DRIVE-CLiQ with 24 V Connector RJ45 IP20 on module side and IP67 on motor side MOTION-CONNECT 800PLUS released only up to 75 m length Dmax=7.1 mm Length (m)= 0 + 0 + 5 + 0,2",192,"ΤΕΜ",1,"MC",1,"6FX80022DC101AF2"]
["6FX8002-2DC10-1CH0","signal cable, pre-assembled type: 6FX8002-2DC10 DRIVE-CLiQ with 24 V Connector RJ45 IP20 on module side and IP67 on motor side MOTION-CONNECT 800PLUS released only up to 75 m length Dmax=7.1 mm Length (m)= 0 + 20 + 7 + 0",381,"ΤΕΜ",1,"MC",1,"6FX80022DC101CH0"]
["6FX8002-2DC20-1CC0","Signal cable pre-assembled type: 6FX8002-2DC20 DRIVE-CLiQ with 24 V Connector RJ45 IP67 on both sides released only up to 75 m length Dmax=7.1 mm Length (m)= 0 + 20 + 2 + 0",358,"ΤΕΜ",1,"MC",1,"6FX80022DC201CC0"]
["6FX8002-2DC36-1BA0","Signal cable pre-assembled type: 6FX8002-2DC36 DRIVE-CLiQ with 24 V M12 female/ RJ45 IP67 MOTION-CONNECT 800PLUS UL/CSA, DESINA, Trailable Dmax=7.1 mm Length (m)=10",262,"ΤΕΜ",1,"MC",1,"6FX80022DC361BA0"]
["6FX8002-2DC42-1BE0","Signal cable pre-assembled type: 6FX8002-2DC42 DRIVE-CLiQ with 24 V RJ45 IP67/M17 male Speed-connect-ready MOTION-CONNECT 800PLUS UL/CSA, DESINA, Trailable Dmax=7.1 mm Length (m)= 0 + 10 + 4 + 0",323,"ΤΕΜ",1,"MC",1,"6FX80022DC421BE0"]
["6FX8002-2EQ10-1AH0","Signal cable pre-assembled for absolute encoder EnDat integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2EQ10 LENGTH (M) = 0 + 0 + 7 + 0",240,"ΤΕΜ",1,"MC",1,"6FX80022EQ101AH0"]
["6FX8002-2EQ14-1DA0","Signal cable extension for base 6FX8002-2EQ10-.... 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8002-2EQ14 LENGTH (M) = 0 + 30 + 0 + 0",533,"ΤΕΜ",1,"MC",1,"6FX80022EQ141DA0"]
["6FX8002-2FN24-1AF8","Signal cable extension for base 6FX.002-2FN20-.... SPEED-CONNECT M17 3x 2x 0.14+4x 0.14 C MOTION-CONNECT 800 trailable, UL/CSA, DESINA Dmax=9.2 mm TYPE: 6FX8002-2FN24 LENGTH (M) = 0 + 0 + 5 + 0,8",299,"ΤΕΜ",1,"MC",1,"6FX80022FN241AF8"]
["6FX8002-2YW11-1AJ7","Signal cable pre-assembled type: 6FX8002-2YW11 Customer-specific Length (m)=8.7",476,"ΤΕΜ",1,"MC",1,"6FX80022YW111AJ7"]
["6FX8002-5CA38-1AG0","power cable extension 4x 2.5 C Connector full thread Sz. 1.5 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=11 mm Length (m)= TYPE: 6FX8002-5CA38 LENGTH (M) = 0 + 0 + 6 + 0",520,"ΤΕΜ",1,"MC",1,"6FX80025CA381AG0"]
["6FX8002-5CA68-1AJ0","power cable extension 4x 10 C Connector full thread Sz. 1.5 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=18.2 mm Length (m)= TYPE: 6FX8002-5CA68 LENGTH (M) = 0 + 0 + 8 + 0",753,"ΤΕΜ",1,"MC",1,"6FX80025CA681AJ0"]
["6FX8002-5CG10-1AB8","Power cable pre-assembled 4x 1.5 C, SPEED-CONNECT Sz. 1 for SINAMICS S120 Power Module MOTION-CONNECT 800PLUS Trailable UL/CSA, DESINA Dmax=9.5 mm, Length (m)= TYPE: 6FX8002-5CG10 LENGTH (M) = + 0 + 0 + 1 + 0,8",170,"ΤΕΜ",1,"MC",1,"6FX80025CG101AB8"]
["6FX8002-5CG41-1AK5","Power cable pre-assembled type: 6FX8002-5CG41 4x 4 C Connector full thread Sz. 1.5 for SINAMICS S120 Power Module and Motor Module Booksize Compact MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=12.3 mm Length (m)= + 0 + 0 + 9 + 0,5",434,"ΤΕΜ",1,"MC",1,"6FX80025CG411AK5"]
["6FX8002-5CN06-1CC5","Power cable pre-assembled TYPE 6FX8002-5CN06 4X1,5 C, SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=9.5 MM LENGTH (M) = + 0 + 20 + 2 + 0.5",483,"ΤΕΜ",1,"MC",1,"6FX80025CN061CC5"]
["6FX8002-5CN36-1CD0","Power cable pre-assembled TYPE 6FX8002-5CN36 4X2.5 C CONNECTOR SPEED-CONNECT S. 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=11 MM LENGTH (M) = + 0 + 20 + 3 + 0",589,"ΤΕΜ",1,"MC",1,"6FX80025CN361CD0"]
["6FX8002-5CN56-1CC0","Power cable pre-assembled TYPE 6FX8002-5CN56 4X6 C CONNECTOR SPEED-CONNECT S. 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=14.9 MM LENGTH (M) = + 0 + 20 + 2 + 0",749,"ΤΕΜ",1,"MC",1,"6FX80025CN561CC0"]
["6FX8002-5CR21-1BF0","Power cable pre-assembled type: 6FX8002-5CR21 4x 4 C Screw connection M32/1PH810. for SINAMICS S120 Power Module and Motor Mod. Booksize Compact MOTION-CONNECT 800PLUS UL/CSA, DESINA Dmax=12.3 mm Length (m)= 0 + 10 + 5 + 0",559,"ΤΕΜ",1,"MC",1,"6FX80025CR211BF0"]
["6FX8002-5CR53-1BF0","Power cable pre-assembled type: 6FX8002-5CR53 4x 16 C Screw connection M50/1PH813 for SINAMICS S120, with bare core ends at module side MOTION-CONNECT 800PLUS Dmax=22.3 mm Length (m)= 0 + 10 + 5 + 0",1072,"ΤΕΜ",1,"MC",1,"6FX80025CR531BF0"]
["6FX8002-5CS14-1BD0","Power cable pre-assembled type: 6FX8002-5CS14 (1FT/1FK/for SINAMICS) 4x 10 C, Connector size 3 Ring cable lugs UL/CSA DESINA, Trailable MOTION-CONNECT 800 Dmax=19.4 mm; Length (m)= 0 + 10 + 3 + 0",976,"ΤΕΜ",1,"MC",1,"6FX80025CS141BD0"]
["6FX8002-5CS54-1CG0","Power cable pre-assembled type: 6FX8002-5CS54 4x 6 C Connector full thread Sz. 1.5 Ring cable lugs on module side for SINAMICS S120 Motor Module MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=14.9 mm Length (m)= 0 + 20 + 6 + 0",928,"ΤΕΜ",1,"MC",1,"6FX80025CS541CG0"]
["6FX8002-5CX28-1BD0","power cable extension 4x 16 C Connector full thread Sz. 3 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=22.3 mm Length (m)= TYPE: 6FX8002-5CX28 LENGTH (M) = 0 + 10 + 3 + 0",2438,"ΤΕΜ",1,"MC",1,"6FX80025CX281BD0"]
["6FX8002-5DA15-1BA0","power cable extension 4x 2.5+(2x1.5) C C MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=13.8 mm Length (m)= TYPE: 6FX8002-5DA15 LENGTH (M) = 0 + 10 + 0 + 0",485,"ΤΕΜ",1,"MC",1,"6FX80025DA151BA0"]
["6FX8002-5DA38-1CJ0","power cable extension 4x 2.5+(2x1.5) C C Connector full thread Sz. 1.5 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=13.8 mm Length (m)= TYPE: 6FX8002-5DA38 LENGTH (M) = 0 + 20 + 8 + 0",1016,"ΤΕΜ",1,"MC",1,"6FX80025DA381CJ0"]
["6FX8002-5DG01-1FA0","Power cable pre-assembled type: 6FX8002-5DG01 4x 1.5+(2x1.5) C C, connector Connector full thread Sz. 1 for SINAMICS Power Module MOTION-CONNECT 800PLUS Dmax=12 mm, Length (m)= + 0 + 50 + 0 + 0",1056,"ΤΕΜ",1,"MC",1,"6FX80025DG011FA0"]
["6FX8002-5DG21-1CA0","Power cable pre-assembled type: 6FX8002-5DG21 4x 1.5+(2x1.5) C C, connector Connector full thread Sz. 1.5 for SINAMICS Power Module MOTION-CONNECT 800PLUS Dmax=12 mm, Length (m)= 0 + 20 + 0 + 0",603,"ΤΕΜ",1,"MC",1,"6FX80025DG211CA0"]
["6FX8002-5DG31-1CF0","Power cable pre-assembled type: 6FX8002-5DG31 4x 2.5+(2x1.5) C C Connector full thread Sz. 1.5 for SINAMICS S120 Power Module and Motor Mod. Booksize Compact MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=13.8 mm Length (m)= + 0 + 20 + 5 + 0",760,"ΤΕΜ",1,"MC",1,"6FX80025DG311CF0"]
["6FX8002-5DG43-1GF0","Power cable pre-assembled type: 6FX8002-5DG43 (motors for Power Module and Motor Module) 4x 35+(2x1.5) C, Connector size 3 Core end cut off Length 300 mm UL/CSA DESINA MOTION-CONNECT 800 Dmax=32.0 mm Length (m)= Accessory kit: 4x cable lugs M8 1x cable lugs M6 1x spring-loaded terminal 0 + 60 + 5 + 0",9830,"ΤΕΜ",1,"MC",1,"6FX80025DG431GF0"]
["6FX8002-5DN16-1BK0","Power cable pre-assembled TYPE 6FX8002-5DN16 4X2.5 , (2X1.5)C C CONNECTOR SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=13.8 MM LENGTH (M) = + 0 + 10 + 9 + 0",563,"ΤΕΜ",1,"MC",1,"6FX80025DN161BK0"]
["6FX8002-5DN36-1BB0","Power cable pre-assembled TYPE 6FX8002-5DN36 4X2.5 , (2X1.5)C C CONNECTOR SPEED-CONNECT S. 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=13.8 MM LENGTH (M) = + 0 + 10 + 1 + 0",492,"ΤΕΜ",1,"MC",1,"6FX80025DN361BB0"]
["6FX8002-5DQ28-1AJ0","power cable extension 4x 1.5+(2x1.5) C C, connector SPEED-CONNECT Sz. 1.5 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=12 mm, Length (m)= TYPE: 6FX8002-5DQ28 LENGTH (M) = + 0 + 0 + 8 + 0",577,"ΤΕΜ",1,"MC",1,"6FX80025DQ281AJ0"]
["6FX8002-5DQ38-1BD0","power cable extension 4x 2.5+(2x1.5) C C SPEED-CONNECT connector Sz. 1.5 MOTION-CONNECT 800PLUS Trailable UL/CSA, DESINA Dmax=13.9 mm Length (m)= TYPE: 6FX8002-5DQ38 LENGTH (M) = + 0 + 10 + 3 + 0",706,"ΤΕΜ",1,"MC",1,"6FX80025DQ381BD0"]
["6FX8002-5DS16-1CJ0","Power cable pre-assembled TYPE 6FX8002-5DS16 4X2.5 , (2X1.5)C C CONNECTOR FULL THREAD SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=13.8 MM LENGTH (M) = + 0 + 20 + 8 + 0",716,"ΤΕΜ",1,"MC",1,"6FX80025DS161CJ0"]
["6FX8002-5DS46-1EA0","Power cable pre-assembled TYPE 6FX8002-5DS46 4X4, (2X1.5)C C CONNECTOR FULL THREAD SIZE 1.5 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=15.2 MM LENGTH (M) = + 0 + 40 + 0 + 0",1124,"ΤΕΜ",1,"MC",1,"6FX80025DS461EA0"]
["6FX8002-5DX28-1AC0","power cable extension 4x 16+(2x1.5) C C Connector full thread Sz. 3 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=23.8 mm Length (m)= TYPE: 6FX8002-5DX28 LENGTH (M) = 0 + 0 + 2 + 0",1993,"ΤΕΜ",1,"MC",1,"6FX80025DX281AC0"]
["6FX8002-5YT05-1BB0","Power cable pre-assembled type: 6FX8002-5YT05 Customer-specific Length (m)= 0 + 10 + 1 + 0",617,"ΤΕΜ",1,"MC",1,"6FX80025YT051BB0"]
["6FX8002-7HY00-1BF0","Pre-assembled hybrid cable type: 6FX8002-7HY00 Power and DRIVE-CLiQ Outlet direction NDE/NDE for SINAMICS S120M MOTION-CONNECT 800PLUS Trailing type, UL/CSA DESINA Dmax=15 mm, Length (m)= 0 + 10 + 5 + 0",798,"ΤΕΜ",1,"MC",1,"6FX80027HY001BF0"]
["6FX8002-7HY22-1AB0","Pre-assembled hybrid cable type: 6FX8002-7HY22 Power and DRIVE-CLiQ Outlet direction DE/DE for SINAMICS S120M MOTION-CONNECT 800PLUS Trailing type, UL/CSA DESINA Dmax=15 mm, Length (m)= 0 + 0 + 1 + 0",439,"ΤΕΜ",1,"MC",1,"6FX80027HY221AB0"]
["6FX8008-1BA25-1BH0","Power cable sold by the meter type: 6FX8008-1BA25 4x 25+(2x1.5) C C MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=27.6 mm Type of delivery: up to 19 m ring from 20 m drum Length (m)= 0 + 10 + 7 + 0",1957,"ΤΕΜ",1,"MC",1,"6FX80081BA251BH0"]
["6FX8008-1BA50-1AF0","Power cable sold by the meter type: 6FX8008-1BA50 4x 50+(2x1.5) C C MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=35 mm Type of delivery: to 9 m ring from 10 m drum Length (m)= 0 + 0 + 5 + 0",1045,"ΤΕΜ",1,"MC",1,"6FX80081BA501AF0"]
["6FX8008-1BB41-1BB0","Power cable sold by the meter type: 6FX8008-1BB41 4x 6.0 C trailable UL/CSA DESINA MOTION-CONNECT 800PLUS Type of delivery: to 69 m ring from 70 m drum Dmax=14.9 mm, Length (m)= 0 + 10 + 1 + 0",317,"ΤΕΜ",1,"MC",1,"6FX80081BB411BB0"]
["6FX8008-1BB41-3AA0","Power cable sold by the meter type: 6FX8008-1BB41 4x 6.0 C trailable UL/CSA DESINA MOTION-CONNECT 800PLUS Type of delivery: to 69 m ring from 70 m drum Dmax=14.9 mm, Length (m)= 200 + 0 + 0 + 0",5481,"ΤΕΜ",1,"MC",1,"6FX80081BB413AA0"]
["6FX8012-2CA31-1AH0","Signal cable pre-assembled for incr. encoder with C/D tracks integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C Connector full thread M23 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8012-2CA31 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = + 0 + 0 + 7 + 0",241,"ΤΕΜ",1,"MC",1,"6FX80122CA311AH0"]
["6FX8012-2EQ31-1AJ0","Signal cable pre-assembled for absolute encoder EnDat integrated into the motor 3x (2x0.14) C+4x 0.14+2x0.5 +4x 0.22 C SPEED-CONNECT connector M23 MOTION-CONNECT 800PLUS trailable, UL/CSA, DESINA Dmax=9.8 mm Length (m)= TYPE: 6FX8012-2EQ31 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = + 0 + 0 + 8 + 0",252,"ΤΕΜ",1,"MC",1,"6FX80122EQ311AJ0"]
["6FX8012-5DA05-1BD0","power cable extension 4x 1.5+(2x1.5) C, connector Full-thread, size 1 MOTION-CONNECT 800PLUS trailable UL/CSA DESINA Dmax=12 mm, LONGUEUR (m)= TYPE: 6FX8012-5DA05 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = 0 + 10 + 3 + 0",509,"ΤΕΜ",1,"MC",1,"6FX80125DA051BD0"]
["6FX8022-5CN06-1CE0","Power cable pre-assembled TYPE 6FX8022-5CN06 4X1,5 C, SPEED-CONNECT SIZE 1 FOR SINAMICS S120 BOOKSIZE MOTOR MODULE C-/D-TYPES PREPARED CONDUCTORS, W/O SINAMICS CONNECTOR MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=9.5 MM LENGTH (M) = + 0 + 20 + 4 + 0",462,"ΤΕΜ",1,"MC",1,"6FX80225CN061CE0"]
["6RA8000-0MS20-0AA0","SINAMICS DCM Control Module Version for power plant excitation systems THYRIPOL",6500,"ΤΕΜ",1,"MC",1,"6RA80000MS200AA0"]
["6RA8075-6GV62-0AA0","SINAMICS DCM DC converter for 4-quadrant drives Circuit (B6) A (B6) C Input: 575V 3AC, 174A controllable: Field rectifier D600/210 MREQ-GEGF6V62 Output: 600 V DC, 210 A",7919,"ΤΕΜ",1,"MC",1,"6RA80756GV620AA0"]
["6RX1800-4GK01","Commutating reactor for converter; Phases: 3 F(Hz): 50/60; ILN=Ithmax(A): 106 UN(V): 575 (50Hz)/690 (60Hz) UK (%): 4; Lrated (mH): 0.399 tA/insulating material class: 40Β°/B; IP00 connection: Terminal connection EN 61558-2-20",2586,"ΤΕΜ",1,"MC",1,"6RX18004GK01"]
["6SL3000-2CE34-1AA0","SINAMICS/MICROMASTER PX LC-MOTOR FILTER FOR 3-PH. 380-480V, 50/60 HZ, 490 A AC DRIVE/POWER MODULE/ MOTOR MODULE",10155,"ΤΕΜ",1,"MC",1,"6SL30002CE341AA0"]
["6SL3000-2DE38-4AA0","SINAMICS DU/DT filter plus Voltage peak limiter for Power Module/Motor Module 450kW, 380-480V 3AC max. cable length 300/450 m",15830,"ΤΕΜ",1,"MC",1,"6SL30002DE384AA0"]
["6SL3070-0BB03-0AA8","SINAMICS ENGINEERING SYSTEM SINAMICS DCB STUDIO SOURCE CODE V1.1 (CONTAINED OPEN-SOURCE-SOFTWARE FREE OF CHARGE) DELIVERY ON DATA CARRIER DVD CUSTOMER-SPECIFIC DELIVERY RELEASE !",125,"ΤΕΜ",1,"MC",1,"6SL30700BB030AA8"]
["6SL3097-0AT00-0AP0","SINAMICS S120 DOCUMENTATION SYSTEM MANUAL CONTROL CABINET INTEGRATION EDITION 09/07, GERMAN",24.5,"ΤΕΜ",1,"MC",1,"6SL30970AT000AP0"]
["6SL3097-5AL00-0CP1","SINAMICS S120 documentation AC Drive Equipment manual Edition 06/19, Italian",187,"ΤΕΜ",1,"MC",1,"6SL30975AL000CP1"]
["6SL3111-4VE21-6EC1","SINAMICS S120 Combi B01 Power Module Input: 400 V 3 AC, 16 kW Output: 400 V 3 AC, 24 A, 12 A, 9 A, 9 A Design: Combi External air cooling Support of the extended Safety Integrated function",7722,"ΤΕΜ",1,"MC",1,"6SL31114VE216EC1"]
["6SL3130-7TE25-5AA3","SINAMICS S120 ACTIVE LINE MODULE INPUT: 3AC 380-480V, 50/60HZ OUTPUT: DC 600V, 92A, 55KW FRAME SIZE: BOOKSIZE INTERNAL AIR COOLING INCL. DRIVE-CLIQ CABLE",7152,"ΤΕΜ",1,"MC",1,"6SL31307TE255AA3"]
["6SL3210-1KE13-2UB2","SINAMICS G120C RATED POWER 1,1KW WITH 150% OVERLOAD FOR 3 SEC 3AC380-480V +10/-20% 47-63HZ UNFILTERED I/O-INTERFACE: 6DI, 2DO,1AI,1AO SAFE TORQUE OFF INTEGRATED FIELDBUS: USS/ MODBUS RTU PROTECTION: IP20/ UL OPEN TYPE SIZE: FSAA 173X73X155(HXWXD) EXTERNAL 24V",619,"ΤΕΜ",1,"MC",1,"6SL32101KE132UB2"]
["6SL3210-1KE18-8AF1","SINAMICS G120C RATED POWER 4,0KW WITH 150% OVERLOAD FOR 3 SEC 3AC380-480V +10/-20% 47-63HZ INTEGRATED FILTER CLASS A I/O-INTERFACE: 6DI, 2DO,1AI,1AO SAFE TORQUE OFF INTEGRATED FIELDBUS: PROFINET-PN PROTECTION: IP20/ UL OPEN TYPE SIZE: FSA 196X73X225,4(HXWXD) EXTERNAL 24V",1207,"ΤΕΜ",1,"MC",1,"6SL32101KE188AF1"]
["6SL3210-1PE12-3AL1","SINAMICS Power Module PM240-2 with integrated Class A filter with integrated braking chopper 380-480 V 3 AC +10/-10% 47-63 Hz Power high overload: 0.55kW at 200% 3s, 150% 57s, 100% 240 s; Ambient temperature -10 to +50 Β°C; power low overload: 0.75kW at 150% 3s, 110% 57s, 100% 240 s; Ambient temperature -10 to +40 Β°C 196x 73x 165 (HxWxD), FSA Degree of protection IP20 without Control Unit and operating unit Released as of CU firmware version V4.6",481,"ΤΕΜ",1,"MC",1,"6SL32101PE123AL1"]
["6SL3210-1RE31-1AL0","SINAMICS G120 POWER MODULE PM240P-2 WITH BUILT IN CL. A FILTER 3AC380-480V +10/-20% 47-63HZ OUTPUT HIGH OVERLOAD: 45KW FOR 150% 60S, 100% 240S; AMBIENT TEMP -20 TO +50 DEG C (HO) OUTPUT LOW OVERLOAD: 55kW FOR 135% 3S,110% 57S,100% 240S AMBIENT TEMP -20 TO +40 DEG C (LO) 551x 275x 237 (HXWXD), FSE PROTECTION IP20 WITHOUT CONTROL UNIT AND PANEL APPROVED FOR CU FIRMWARE- VERSION V4.7 SP6 HF1",6971,"ΤΕΜ",1,"MC",1,"6SL32101RE311AL0"]
["6SL3220-1YC18-1UP0","SINAMICS G120X Rated power: 3 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSB Degree of protection IP20 / UL open type painting 3C2 without operator panel with IO expansions Fieldbus integrated: PROFIBUS DP",902,"ΤΕΜ",1,"MC",1,"6SL32201YC181UP0"]
["6SL3220-1YC40-0UP0","SINAMICS G120X Rated power: 55 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSF Degree of protection IP20 / UL open type painting 3C2 without operator panel Without IO expansion Fieldbus integrated: PROFIBUS DP",6486,"ΤΕΜ",1,"MC",1,"6SL32201YC400UP0"]
["6SL3220-1YE22-0UP0","SINAMICS G120X Rated power: 5.5 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSB Degree of protection IP20 / UL open type painting 3C2 without operator panel Without IO expansion Fieldbus integrated: PROFIBUS DP",1106,"ΤΕΜ",1,"MC",1,"6SL32201YE220UP0"]
["6SL3220-1YE46-1AF0","SINAMICS G120X Rated power: 110 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSF Degree of protection IP20 / UL open type painting 3C2 without operator panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",10373,"ΤΕΜ",1,"MC",1,"6SL32201YE461AF0"]
["6SL3220-1YH22-0UF0","SINAMICS G120X Rated power: 5.5 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSD Degree of protection IP20 / UL open type painting 3C2 without operator panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",1355,"ΤΕΜ",1,"MC",1,"6SL32201YH220UF0"]
["6SL3220-1YH36-0AF0","SINAMICS G120X Rated power: 37 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSD Degree of protection IP20 / UL open type painting 3C2 without operator panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",5209,"ΤΕΜ",1,"MC",1,"6SL32201YH360AF0"]
["6SL3220-2YC24-0UP0","SINAMICS G120X Rated power: 7.5 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSC Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel Without IO expansion Fieldbus integrated: PROFIBUS DP",1435,"ΤΕΜ",1,"MC",1,"6SL32202YC240UP0"]
["6SL3220-2YC30-1UP0","SINAMICS G120X Rated power: 18.5 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSD Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel with IO expansions Fieldbus integrated: PROFIBUS DP",2736,"ΤΕΜ",1,"MC",1,"6SL32202YC301UP0"]
["6SL3220-2YE28-0UB0","SINAMICS G120X Rated power: 15 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSC Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",1986,"ΤΕΜ",1,"MC",1,"6SL32202YE280UB0"]
["6SL3220-2YE36-0UF0","SINAMICS G120X Rated power: 37 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSD Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",4260,"ΤΕΜ",1,"MC",1,"6SL32202YE360UF0"]
["6SL3220-2YH24-1UB0","SINAMICS G120X Rated power: 7.5 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSD Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",1573,"ΤΕΜ",1,"MC",1,"6SL32202YH241UB0"]
["6SL3220-2YH36-0UB0","SINAMICS G120X Rated power: 37 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSD Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",4759,"ΤΕΜ",1,"MC",1,"6SL32202YH360UB0"]
["6SL3220-2YH50-0CB0","SINAMICS G120X Rated power: 160 kW At 110% 60s, 100% 240 s Radio interference suppression filter For category C3 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSG Degree of protection IP20 / UL open type painting 3C2 with Basic Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",14230,"ΤΕΜ",1,"MC",1,"6SL32202YH500CB0"]
["6SL3220-3YC40-0UB0","SINAMICS G120X rated power: 55 kW at 110% 60s, 100% 240s unfiltered 200-240V3AC+10/-20% 47-63Hz ambient temperature -20 to +45 Β°C frame size: FSF degree of protection IP20 / UL open type painting 3C2 with Intelligent Operator Panel without IO expansion fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",6520,"ΤΕΜ",1,"MC",1,"6SL32203YC400UB0"]
["6SL3220-3YE28-0UP0","SINAMICS G120X rated power: 15 kW at 110% 60s, 100% 240s unfiltered 380-480V3AC+10/-20% 47-63Hz ambient temperature -20 to +45 Β°C frame size: FSC degree of protection IP20 / UL open type painting 3C2 with Intelligent Operator Panel without IO expansion fieldbus integrated: PROFIBUS DP",2210,"ΤΕΜ",1,"MC",1,"6SL32203YE280UP0"]
["6SL3220-3YE42-0AP0","SINAMICS G120X Rated power: 75 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSF Degree of protection IP20 / UL open type painting 3C2 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: PROFIBUS DP",7776,"ΤΕΜ",1,"MC",1,"6SL32203YE420AP0"]
["6SL3220-3YE50-0CB0","SINAMICS G120X Rated power: 160 kW At 110% 60s, 100% 240 s Radio interference suppression filter For category C3 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSG Degree of protection IP20 / UL open type painting 3C2 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",12472,"ΤΕΜ",1,"MC",1,"6SL32203YE500CB0"]
["6SL3220-3YH30-1UB0","SINAMICS G120X Rated power: 18.5 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSD Degree of protection IP20 / UL open type painting 3C2 With Intelligent Operator Panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",2898,"ΤΕΜ",1,"MC",1,"6SL32203YH301UB0"]
["6SL3223-0DE25-5AG1","SINAMICS G120P Power Module PM230 with integrated Class A filter Degree of protection IP55/UL Type 12 380-480 V 3 AC +10/-10% 47-63 Hz Power low overload: 5.5kW at 150% 3s, 110% 57s, 100% 240 s; Ambient temperature -10 to +40 Β°C (LO) 540x 180x 249 (HxWxD), FSB without Control Unit and operating unit released for CU230P-2 Firmware version V4.3.2 or higher",1227,"ΤΕΜ",1,"MC",1,"6SL32230DE255AG1"]
["6SL3230-1YC12-0UB0","SINAMICS G120X Rated power: 1.1 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSA Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",639,"ΤΕΜ",1,"MC",1,"6SL32301YC120UB0"]
["6SL3230-1YE20-1AP0","SINAMICS G120X Rated power: 4 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSB Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel with IO expansions Fieldbus integrated: PROFIBUS DP",1430,"ΤΕΜ",1,"MC",1,"6SL32301YE201AP0"]
["6SL3230-1YE38-0AF0","SINAMICS G120X Rated power: 45 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSE Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",5751,"ΤΕΜ",1,"MC",1,"6SL32301YE380AF0"]
["6SL3230-1YE46-0AP0","SINAMICS G120X Rated power: 110 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel Without IO expansion Fieldbus integrated: PROFIBUS DP",10768,"ΤΕΜ",1,"MC",1,"6SL32301YE460AP0"]
["6SL3230-1YH24-1UP0","SINAMICS G120X Rated power: 7.5 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel with IO expansions Fieldbus integrated: PROFIBUS DP",1892,"ΤΕΜ",1,"MC",1,"6SL32301YH241UP0"]
["6SL3230-1YH46-0CF0","SINAMICS G120X Rated power: 110 kW At 110% 60s, 100% 240 s Radio interference suppression filter For category C3 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 without operator panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",11891,"ΤΕΜ",1,"MC",1,"6SL32301YH460CF0"]
["6SL3230-2YC22-1UF0","SINAMICS G120X Rated power: 5.5 kW At 110% 60s, 100% 240 s Unfiltered 200-240 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSC Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",1548,"ΤΕΜ",1,"MC",1,"6SL32302YC221UF0"]
["6SL3230-2YE14-0AF0","SINAMICS G120X Rated power: 1.5 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSA Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",1031,"ΤΕΜ",1,"MC",1,"6SL32302YE140AF0"]
["6SL3230-2YE26-1AP0","SINAMICS G120X Rated power: 11 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSC Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel with IO expansions Fieldbus integrated: PROFIBUS DP",2269,"ΤΕΜ",1,"MC",1,"6SL32302YE261AP0"]
["6SL3230-2YE52-0AB0","SINAMICS G120X Rated power: 200 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSG Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",16657,"ΤΕΜ",1,"MC",1,"6SL32302YE520AB0"]
["6SL3230-2YH22-0AF0","SINAMICS G120X Rated power: 5.5 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel Without IO expansion Fieldbus integrated: PROFINET PN, Ethernet IP",1767,"ΤΕΜ",1,"MC",1,"6SL32302YH220AF0"]
["6SL3230-2YH48-0CB0","SINAMICS G120X Rated power: 132 kW At 110% 60s, 100% 240 s Radio interference suppression filter For category C3 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",13193,"ΤΕΜ",1,"MC",1,"6SL32302YH480CB0"]
["6SL3230-2YH48-1CP0","SINAMICS G120X Rated power: 132 kW At 110% 60s, 100% 240 s Radio interference suppression filter For category C3 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSF Degree of protection IP20 / UL open type Paint finish 3C3 with Basic Operator Panel with IO expansions Fieldbus integrated: PROFIBUS DP",13409,"ΤΕΜ",1,"MC",1,"6SL32302YH481CP0"]
["6SL3230-3YE14-0UB0","SINAMICS G120X Rated power: 1.5 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSA Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel Without IO expansion Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",938,"ΤΕΜ",1,"MC",1,"6SL32303YE140UB0"]
["6SL3230-3YE30-1UB0","SINAMICS G120X Rated power: 18.5 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel with IO expansions Fieldbus integrated: MODBUS RTU, BACnet MS/TP,USS",2866,"ΤΕΜ",1,"MC",1,"6SL32303YE301UB0"]
["6SL3230-3YE40-1UF0","SINAMICS G120X Rated power: 55 kW At 110% 60s, 100% 240 s Unfiltered 380-480 V 3 AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSE Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel with IO expansions Fieldbus integrated: PROFINET PN, Ethernet IP",6573,"ΤΕΜ",1,"MC",1,"6SL32303YE401UF0"]
["6SL3230-3YH26-1UP0","SINAMICS G120X Rated power: 11 kW At 110% 60s, 100% 240 s Unfiltered 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSD Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel with IO expansions Fieldbus integrated: PROFIBUS DP",2389,"ΤΕΜ",1,"MC",1,"6SL32303YH261UP0"]
["6SL3230-3YH40-1AP0","SINAMICS G120X Rated power: 55 kW At 110% 60s, 100% 240 s Radio interference suppression filter for category C2 500-690 V 3AC +10/-20% 47-63 Hz Ambient temperature -20 to +45 Β°C Size: FSE Degree of protection IP20 / UL open type Paint finish 3C3 With Intelligent Operator Panel with IO expansions Fieldbus integrated: PROFIBUS DP",7976,"ΤΕΜ",1,"MC",1,"6SL32303YH401AP0"]
["6SL3244-0BB12-1FA0","SINAMICS G120 CONTROL UNIT CU240E-2 PN E-TYPE SAFETY INTEGRATED STO PROFINET 6DI, 3DO, 2AI, 2AO, MAX 1F-DI PTC/KTY INTERFACE USB- AND SD/MMC-INTERFACE PROTECTION IP20 AMBIENT TEMP 0 TO +50 DEG C WITHOUT POWER MODULE AND PANEL",432,"ΤΕΜ",1,"MC",1,"6SL32440BB121FA0"]
["6SL3325-1TE33-1AA3","SINAMICS S120 SINGLE MOTOR MODULES INPUT: 600 V DC OUTPUT: 3-PH 400 V, 310 A FRAME SIZE: CHASSIS LIQUID COOLING SUPPORT OF EXTENDED SAFETY INTEGRATED FUNCTIONS",27803,"ΤΕΜ",1,"MC",1,"6SL33251TE331AA3"]
["6SL3520-0XA21-5AF0","SINAMICS G115D wall-mounted Rated power: 1.5kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC without operation option with cable gland with communication Fieldbus integrated: PROFINET PN, Ethernet IP",1258,"ΤΕΜ",1,"MC",1,"6SL35200XA215AF0"]
["6SL3520-0XA61-5AA0","SINAMICS G115D wall-mounted Rated power: 1.5kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC without operation option with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication fieldbus integrated: AS-Interface",1135,"ΤΕΜ",1,"MC",1,"6SL35200XA615AA0"]
["6SL3520-0XD01-1AB0","SINAMICS G115D wall-mounted Rated power: 1.1 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC without operation option with MQ(X)15 for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication without looping through Q8/0 for motor connection without fieldbus",970,"ΤΕΜ",1,"MC",1,"6SL35200XD011AB0"]
["6SL3520-0XL02-2AF0","SINAMICS G115D wall-mounted Rated power: 2.2 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC without operation option Quickon for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through Fieldbus integrated: PROFINET PN, Ethernet IP",1827,"ΤΕΜ",1,"MC",1,"6SL35200XL022AF0"]
["6SL3520-0XN05-5AA0","SINAMICS G115D wall-mounted Rated power: 5.5 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSC Protection class IP65/66 / UL Type 4X brake voltage 180 V DC without operation option Q4/2 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU with looping through fieldbus integrated: AS-Interface",2494,"ΤΕΜ",1,"MC",1,"6SL35200XN055AA0"]
["6SL3520-1XA67-5AB0","SINAMICS G115D wall-mounted Rated power: 7.5 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSC Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication without fieldbus",2532,"ΤΕΜ",1,"MC",1,"6SL35201XA675AB0"]
["6SL3520-1XE40-5AF0","SINAMICS G115D wall-mounted Rated power: 0.55 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch Q4/2 for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication with looping through Q8/0 for motor connection Fieldbus integrated: PROFINET PN, Ethernet IP",1406,"ΤΕΜ",1,"MC",1,"6SL35201XE405AF0"]
["6SL3520-1XK00-5AB0","SINAMICS G115D wall-mounted Rated power: 0.55 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch Q4/2 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through without fieldbus",1122,"ΤΕΜ",1,"MC",1,"6SL35201XK005AB0"]
["6SL3520-1XL01-5AA0","SINAMICS G115D wall-mounted Rated power: 1.5kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch Quickon for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through fieldbus integrated: AS-Interface",1551,"ΤΕΜ",1,"MC",1,"6SL35201XL015AA0"]
["6SL3520-2XA20-7AF0","SINAMICS G115D wall-mounted Rated power: 0.75 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC local remote control with cable gland with communication Fieldbus integrated: PROFINET PN, Ethernet IP",1236,"ΤΕΜ",1,"MC",1,"6SL35202XA207AF0"]
["6SL3520-2XE04-0AB0","SINAMICS G115D wall-mounted Rated power: 4 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC local remote control Q4/2 for 400 V AC and 7/8\" for 24 V DC and M12 for I/O and communication with looping through Q8/0 for motor connection without fieldbus",1883,"ΤΕΜ",1,"MC",1,"6SL35202XE040AB0"]
["6SL3520-2XE43-0AB0","SINAMICS G115D wall-mounted Rated power: 3 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 180 V DC local remote control Q4/2 for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication with looping through Q8/0 for motor connection without fieldbus",1626,"ΤΕΜ",1,"MC",1,"6SL35202XE430AB0"]
["6SL3520-2XL01-5AB0","SINAMICS G115D wall-mounted Rated power: 1.5kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC local remote control Quickon for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through without fieldbus",1391,"ΤΕΜ",1,"MC",1,"6SL35202XL015AB0"]
["6SL3520-3XA01-5AB0","SINAMICS G115D wall-mounted Rated power: 1.5kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch local remote control with cable gland without communication without fieldbus",1112,"ΤΕΜ",1,"MC",1,"6SL35203XA015AB0"]
["6SL3520-3XD01-1AA0","SINAMICS G115D wall-mounted Rated power: 1.1 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch local remote control with MQ(X)15 for 400 V AC and M12 for I/O and communication without looping through Q8/0 for motor connection fieldbus integrated: AS-Interface",1446,"ΤΕΜ",1,"MC",1,"6SL35203XD011AA0"]
["6SL3520-3XH21-1AF0","SINAMICS G115D wall-mounted Rated power: 1.1 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch local remote control with cable gland with communication with integrated 24 V DC PSU Fieldbus integrated: PROFINET PN, Ethernet IP",1617,"ΤΕΜ",1,"MC",1,"6SL35203XH211AF0"]
["6SL3520-3XL00-3AF0","SINAMICS G115D wall-mounted Rated power: 0.37 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 180 V DC repair switch local remote control Quickon for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through Fieldbus integrated: PROFINET PN, Ethernet IP",1667,"ΤΕΜ",1,"MC",1,"6SL35203XL003AF0"]
["6SL3521-0XA67-5AA0","SINAMICS G115D wall-mounted Rated power: 7.5 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSC Protection class IP65/66 / UL Type 4X brake voltage 400 V AC without operation option with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication fieldbus integrated: AS-Interface",2878,"ΤΕΜ",1,"MC",1,"6SL35210XA675AA0"]
["6SL3521-0XB40-5AB0","SINAMICS G115D wall-mounted Rated power: 0.55 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC without operation option Q4/2 for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication without looping through Q8/0 for motor connection without fieldbus",1073,"ΤΕΜ",1,"MC",1,"6SL35210XB405AB0"]
["6SL3521-0XE03-0AA0","SINAMICS G115D wall-mounted Rated power: 3 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 400 V AC without operation option Q4/2 for 400 V AC and M12 for I/O and communication with looping through Q8/0 for motor connection fieldbus integrated: AS-Interface",1911,"ΤΕΜ",1,"MC",1,"6SL35210XE030AA0"]
["6SL3521-0XH63-0AB0","SINAMICS G115D wall-mounted Rated power: 3 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 400 V AC without operation option with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication with integrated 24 V DC PSU without fieldbus",1681,"ΤΕΜ",1,"MC",1,"6SL35210XH630AB0"]
["6SL3521-1XA61-5AF0","SINAMICS G115D wall-mounted Rated power: 1.5kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication Fieldbus integrated: PROFINET PN, Ethernet IP",1632,"ΤΕΜ",1,"MC",1,"6SL35211XA615AF0"]
["6SL3521-1XB41-1AB0","SINAMICS G115D wall-mounted Rated power: 1.1 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch Q4/2 for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication without looping through Q8/0 for motor connection without fieldbus",1288,"ΤΕΜ",1,"MC",1,"6SL35211XB411AB0"]
["6SL3521-1XE00-7AB0","SINAMICS G115D wall-mounted Rated power: 0.75 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch Q4/2 for 400 V AC and 7/8\" for 24 V DC and M12 for I/O and communication with looping through Q8/0 for motor connection without fieldbus",1254,"ΤΕΜ",1,"MC",1,"6SL35211XE007AB0"]
["6SL3521-1XH60-7AF0","SINAMICS G115D wall-mounted Rated power: 0.75 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication with integrated 24 V DC PSU Fieldbus integrated: PROFINET PN, Ethernet IP",1646,"ΤΕΜ",1,"MC",1,"6SL35211XH607AF0"]
["6SL3521-2XA04-0AB0","SINAMICS G115D wall-mounted Rated power: 4 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 400 V AC local remote control with cable gland without communication without fieldbus",1845,"ΤΕΜ",1,"MC",1,"6SL35212XA040AB0"]
["6SL3521-2XB05-5AB0","SINAMICS G115D wall-mounted Rated power: 5.5 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSC Protection class IP65/66 / UL Type 4X brake voltage 400 V AC local remote control Q4/2 for 400 V AC and 7/8\" for 24 V DC and M12 for I/O and communication without looping through Q8/0 for motor connection without fieldbus",2449,"ΤΕΜ",1,"MC",1,"6SL35212XB055AB0"]
["6SL3521-2XH20-3AA0","SINAMICS G115D wall-mounted Rated power: 0.37 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC local remote control with cable gland with communication with integrated 24 V DC PSU fieldbus integrated: AS-Interface",1430,"ΤΕΜ",1,"MC",1,"6SL35212XH203AA0"]
["6SL3521-2XH61-5AA0","SINAMICS G115D wall-mounted Rated power: 1.5kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC local remote control with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication with integrated 24 V DC PSU fieldbus integrated: AS-Interface",1707,"ΤΕΜ",1,"MC",1,"6SL35212XH615AA0"]
["6SL3521-2XN04-0AF0","SINAMICS G115D wall-mounted Rated power: 4 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 400 V AC local remote control Q4/2 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU with looping through Fieldbus integrated: PROFINET PN, Ethernet IP",2651,"ΤΕΜ",1,"MC",1,"6SL35212XN040AF0"]
["6SL3521-3XA61-5AA0","SINAMICS G115D wall-mounted Rated power: 1.5kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch local remote control with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication fieldbus integrated: AS-Interface",1610,"ΤΕΜ",1,"MC",1,"6SL35213XA615AA0"]
["6SL3521-3XE44-0AB0","SINAMICS G115D wall-mounted Rated power: 4 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch local remote control Q4/2 for 400 V AC and Power M12 for 24 V DC and M12 for I/O and communication with looping through Q8/0 for motor connection without fieldbus",2201,"ΤΕΜ",1,"MC",1,"6SL35213XE440AB0"]
["6SL3521-3XH63-0AB0","SINAMICS G115D wall-mounted Rated power: 3 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSB Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch local remote control with cable gland for 400 V AC and 24 V DC and M12 for I/O and communication with integrated 24 V DC PSU without fieldbus",1935,"ΤΕΜ",1,"MC",1,"6SL35213XH630AB0"]
["6SL3521-3XM01-1AB0","SINAMICS G115D wall-mounted Rated power: 1.1 kW for 3S 200%, 57S 150%, 240S 87% Radio interference suppression filter for Cat. C2 3AC380-480V+10/-10% 45-66Hz Ambient temp. -30 to +40Β°C size: FSA Protection class IP65/66 / UL Type 4X brake voltage 400 V AC repair switch local remote control MQ(X)15 for 400 V AC and M12 for I/O and communication with integrated 24 V DC PSU without looping through without fieldbus",1619,"ΤΕΜ",1,"MC",1,"6SL35213XM011AB0"]
["6SL3544-0FB20-1PA0","SINAMICS G120D Control Unit CU240D-2 DP PROFIBUS DP and STO onboard 6 DI/1 F-DI, 2 DO, 2 AI USB interface SD/MMC card interface HTL encoder interface Degree of protection IP65 Ambient temperature -10 to +55 Β°C without Power Module",773,"ΤΕΜ",1,"MC",1,"6SL35440FB201PA0"]
["UAC:FN3440110118E2FAJRX","G120 LINE HARMONICS FILTER 400V 110 kW",8421,"ΤΕΜ",1,"MC",1,"UAC:FN3440110118E2FAJRX"]
["1LE1001-1DA23-4GB4","SIMOTICS GP motor type: 1AV2162A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 160M, * 11 kW (50 Hz) 12.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1601,"ΤΕΜ",1,"LVM",1,"1LE10011DA234GB4"]
["1LE1003-0DA32-2KB4","SIMOTICS GP motor type: 1AV3083A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 2-pole * frame size 80M * 1.1 kW (50 Hz) 1.27 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 14, Standard flange: FT100 (C120) MOTOR PROTECTION WITH 1 PTC THERMISTORS FOR SHUTDOWN Terminal box at top",422,"ΤΕΜ",1,"LVM",1,"1LE10030DA322KB4"]
["1LE1003-1BB22-2JA4","SIMOTICS GP motor type: 1AV3112B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 4-pole * frame size 112M, * 4 kW (50 Hz) 4.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35, flange: FF215 (A250) Without motor protection Terminal box at top",842,"ΤΕΜ",1,"LVM",1,"1LE10031BB222JA4"]
["1LE1004-1DA22-2FB4","SIMOTICS GP motor type: 1AV4162A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 2-pole * frame size 160M, * 11 kW (50 Hz) 12.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2123,"ΤΕΜ",1,"LVM",1,"1LE10041DA222FB4"]
["1LE1023-0EB02-2FA4","SIMOTICS GP motor type: 1AV3090B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure IE3, NEMA Premium, CSA, UL, 4-pole * frame size 90S * 1.1 kW (50 Hz) NEMA 60 Hz: 1.5 HP 60 Hz, P60: IE2 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF165 (A200) without motor protection Terminal box at top",512,"ΤΕΜ",1,"LVM",1,"1LE10230EB022FA4"]
["1LE1501-2DA00-4AA6","SIMOTICS SD motor type: 1CV2280A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 280S, * 75 kW (50 Hz) 84 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box on left-hand side",8737,"ΤΕΜ",1,"LVM",1,"1LE15012DA004AA6"]
["1LE1503-1AA43-4JB6","SIMOTICS SD motor type: 1CV3104A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * frame size 100L * 3 kW (50 Hz) 3.45 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",834,"ΤΕΜ",1,"LVM",1,"1LE15031AA434JB6"]
["1LE1503-1DA30-4AB6","SIMOTICS SD motor type: 1CV3163A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 160M, * 15 kW (50 Hz) 17.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",2435,"ΤΕΜ",1,"LVM",1,"1LE15031DA304AB6"]
["1LE1503-2DA02-2FA4","SIMOTICS SD motor type: 1CV3280A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * frame size 280S, * 75 kW (50 Hz) 84 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF500 (A550) without motor protection Terminal box at top",9193,"ΤΕΜ",1,"LVM",1,"1LE15032DA022FA4"]
["1LE1523-1DA32-2AA4","SIMOTICS SD motor type: 1CV3163A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line IE3, NEMA Premium, CSA, UL, 2-pole * frame size 160M, * 15 kW (50 Hz) NEMA 60 Hz: 20 HP standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, without motor protection Terminal box at top",2546,"ΤΕΜ",1,"LVM",1,"1LE15231DA322AA4"]
["1LE2111-1AB21-4AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR GENERAL PURPOSE GP100A ALUMINUM HOUSING NPP EFFICIENCY TEFC (IP55) 4 POLE * FS 143T 1 HP (60 HZ) 230/460V, 60HZ (suitable for 208V) FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",525,"ΤΕΜ",1,"LVM",1,"1LE21111AB214AA3"]
["1LE2111-2BA11-3AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR GENERAL PURPOSE GP100A ALUMINUM HOUSING NPP EFFICIENCY TEFC (IP55) 2 POLE * FS 254T 15 HP (60 HZ) 575V STD, 60HZ FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",1919,"ΤΕΜ",1,"LVM",1,"1LE21112BA113AA3"]
["1LE2121-1CB11-3AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR GENERAL PURPOSE GP100A ALUMINIUM HOUSING NP EFFICIENCY TEFC (IP55) 4 POLE * FS 182T 3 HP (60 HZ) 575V STD, 60HZ FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",650,"ΤΕΜ",1,"LVM",1,"1LE21211CB113AA3"]
["1LE2211-1CA11-4GA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR GENERAL PURPOSE GP100 CAST-IRON HOUSING NPP EFFICIENCY TEFC (IP55) 2 POLE * FS 182T 3 HP (60 HZ) 230/460V, 60HZ (suitable for 208V) C-FACE W/O FEET WITHOUT WINDING PROTECTION FLOOR F-1",886,"ΤΕΜ",1,"LVM",1,"1LE22111CA114GA3"]
["1LE2211-2BC11-3GA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR GENERAL PURPOSE GP100 CAST-IRON HOUSING NPP EFFICIENCY TEFC (IP55) 6 POLE * FS 254T 7.5 HP (60 HZ) 575V STD, 60HZ C-FACE W/O FEET WITHOUT WINDING PROTECTION FLOOR F-1",2301,"ΤΕΜ",1,"LVM",1,"1LE22112BC113GA3"]
["1LE2221-1AB31-4AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR GENERAL PURPOSE GP100 CAST-IRON HOUSING NP EFFICIENCY TEFC (IP55) 4 POLE * FS 145T 1.5 HP (60 HZ) 230/460V, 60HZ (suitable for 208V) FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",545,"ΤΕΜ",1,"LVM",1,"1LE22211AB314AA3"]
["1LE2221-2AC21-3EA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR GENERAL PURPOSE GP100 CAST-IRON HOUSING NP EFFICIENCY TEFC (IP55) 6 POLE * FS 215T 5 HP (60 HZ) 575V STD, 60HZ C-FACE WITH FEET WITHOUT WINDING PROTECTION FLOOR F-1",1570,"ΤΕΜ",1,"LVM",1,"1LE22212AC213EA3"]
["1LE2221-4DB21-2AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR GENERAL PURPOSE GP100 CAST-IRON HOUSING NP EFFICIENCY TEFC (IP54) 4 POLE *  FS 445TS 150 HP (60 HZ) 460V STD, 60HZ FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",15818,"ΤΕΜ",1,"LVM",1,"1LE22214DB212AA3"]
["1LE2301-4EM24-4AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL-CAGE MOTOR SEVERE DUTY SD10 MS MULTI-SPEED, CAST-IRON HOUSING EPACT EFFICIENCY, TEFC (IP54) 4/8 POLES * FS B445T 125 / 31 HP (60 HZ) 575V Y,YY 1WVT 60HZ FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",21414,"ΤΕΜ",1,"LVM",1,"1LE23014EM244AA3"]
["1LE2321-1AA31-3AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR SEVERE DUTY SD100 CAST-IRON HOUSING NP EFFICIENCY TEFC (IP55) 2 POLE * FS 145T 2 HP (60 HZ) 575V STD, 60HZ FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",756,"ΤΕΜ",1,"LVM",1,"1LE23211AA313AA3"]
["1LE2321-2BC11-3GA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR SEVERE DUTY SD100 CAST-IRON HOUSING NP EFFICIENCY TEFC (IP55) 6 POLE * FS 254T 7.5 HP (60 HZ) 575V STD, 60HZ C-FACE W/O FEET WITHOUT WINDING PROTECTION FLOOR F-1",2239,"ΤΕΜ",1,"LVM",1,"1LE23212BC113GA3"]
["1LE2321-3CC11-3AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR SEVERE DUTY SD100 CAST-IRON HOUSING NP EFFICIENCY TEFC (IP55) 6 POLE *  FS 364T 40 HP (60 HZ) 575V STD, 60HZ FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",7495,"ΤΕΜ",1,"LVM",1,"1LE23213CC113AA3"]
["1LE2321-4CB31-2AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR SEVERE DUTY SD100 CAST-IRON HOUSING BEARING DESIGN FOR INCREASED CANTILEVER FORCES NP EFFICIENCY TEFC (IP55) 4 POLE *  FS 447T 200 HP (60 HZ) 460V, 60HZ FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",23285,"ΤΕΜ",1,"LVM",1,"1LE23214CB312AA3"]
["1LE2411-1AB31-3AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR SEVERE DUTY SD100 IEEE 841, CAST-IRON HOUSING NPP EFFICIENCY TEFC (IP55) 4 POLE * FS 145T 1.5 HP (60 HZ) 575V STD, 60HZ FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",1053,"ΤΕΜ",1,"LVM",1,"1LE24111AB313AA3"]
["1LE2421-1CB11-2GA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR SEVERE DUTY SD100 IEEE 841, CAST-IRON HOUSING NP EFFICIENCY TEFC (IP55) 4 POLE * FS 182T 3 HP (60 HZ) 460V, 60HZ C-FACE W/O FEET WITHOUT WINDING PROTECTION FLOOR F-1",1145,"ΤΕΜ",1,"LVM",1,"1LE24211CB112GA3"]
["1LE2421-2AB21-3AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR SEVERE DUTY SD100 IEEE 841, CAST-IRON HOUSING NP EFFICIENCY TEFC (IP55) 4 POLE * FS 215T 10 HP (60 HZ) 575V STD, 60HZ FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",1820,"ΤΕΜ",1,"LVM",1,"1LE24212AB213AA3"]
["1LE2421-4AB21-2AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR SEVERE DUTY SD100 IEEE 841, CAST-IRON HOUSING NP EFFICIENCY TEFC (IP55) 4 POLE *  FS 405T 100 HP (60 HZ) 460V, 60HZ FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",13990,"ΤΕΜ",1,"LVM",1,"1LE24214AB212AA3"]
["1LE6321-4BB11-2AA1","Low-Voltage Motor, 3 Phase Squirrel Cage, Severe Duty SD200 Cast Iron Housing TEFC (IP55) NP Efficiency, 125HP (60HZ) 4 POLE FS 444T 460V, 60HZ Foot Mounted (F1, F2, F3) Without Winding Protection Terminal box at DE of Motor on LHS viewed from DE (F-1)",16669,"ΤΕΜ",1,"LVM",1,"1LE63214BB112AA1"]
["1LE6321-5EA01-2AA1","Low-Voltage Motor, NEMA Severe Duty SD200 Cast-Iron Housing NP Efficiency TEFC (IP55) 2 Pole * FS 5011S 600 HP (60 HZ) SHORT SHAFT 460 V STD, 60HZ Foot Mounted Horizontal (IMB3 β€“ [F1/F 2/F3]) Without Winding Protection Terminal box at DE of Motor on LHS viewed from DE (F-1)",70723,"ΤΕΜ",1,"LVM",1,"1LE63215EA012AA1"]
["1MB1013-1DC22-2HA4","SIMOTICS XP motor type: 1AV3162C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP65 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3 6-pole * frame size 160M * 7.5 kW (50 Hz) 8.6 kW (60 Hz) version for zone 21 and zone 22 with conductive dust standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V3, flange: FF300 (A350) without motor protection Terminal box at top",2146,"ΤΕΜ",1,"LVM",1,"1MB10131DC222HA4"]
["1MB1513-0EA03-4FB4","SIMOTICS XP motor type: 1CV3090A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP65 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 90S * 1.5 kW (50 Hz), 1.75 kW (60 Hz) Ex tb IIIC T120Β° Db version for zone 21 and zone 22 with conductive dust standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF165 (A200) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",738,"ΤΕΜ",1,"LVM",1,"1MB15130EA034FB4"]
["1MB1533-0DA23-4AB4","SIMOTICS XP motor type: 1CV3082A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 80M * 0.75 kW (50 Hz), 0.88 kW (60 Hz) Ex ec IIC T3 Gc version for zone 2 according to IEC/EN 60 079-7 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",520,"ΤΕΜ",1,"LVM",1,"1MB15330DA234AB4"]
["1MB2121-1AB31-4AG3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR HAZARDOUS DUTY XP100 CAST-IRON HOUSING NP EFFICIENCY, TEFC (IP65) 4 POLE * FS 145T 1.5 HP (60 HZ) CLASS I, GROUPS C&D, DIVISION I CLASS II,GROUPS F&G, DIVISION I 230/460V, 60HZ (SUITABLE FOR 208V) FOOT MOUNTED F-1,2 thermostat FLOOR F-1",1022,"ΤΕΜ",1,"LVM",1,"1MB21211AB314AG3"]
["1MB2121-2BB21-4EG3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR HAZARDOUS DUTY XP100 CAST-IRON HOUSING NP EFFICIENCY, TEFC (IP65) 4 POLE * FS 256T 20 HP (60 HZ) CLASS I, GROUPS C&D, DIVISION I CLASS II,GROUPS F&G, DIVISION I 230/460V, 60HZ (SUITABLE FOR 208V) C-FACE WITH FEET C-1,2; F-1,2; W -1...8 thermostat FLOOR F-1",3835,"ΤΕΜ",1,"LVM",1,"1MB21212BB214EG3"]
["1MB2221-1CC31-4AA3","LOW-VOLTAGE MOTOR, NEMA 3 PHASE SQUIRREL CAGE MOTOR HAZARDOUS DUTY XP100 ID1 CAST-IRON HOUSING NP EFFICIENCY, TEFC (IP65) 6 POLE *  FS 184T 2 HP (60 HZ) CLASS I, GROUP D, DIVISION I 230V/460V, 60Hz (suitable for 208V) FOOT MOUNTED F-1,2 WITHOUT WINDING PROTECTION FLOOR F-1",1221,"ΤΕΜ",1,"LVM",1,"1MB22211CC314AA3"]
["KWA:106575385","*Spare part* Shield DE/NDE ISO4762-4xM16x55 SH 250",381,"ΤΕΜ",1,"LVM",1,"KWA:106575385"]
["KWA:106576889","*Spare part* Retaining ring 85X3",126,"ΤΕΜ",1,"LVM",1,"KWA:106576889"]
["KWA:107161932","spare part Distance Piece 1LE7.3A (AH315)",83,"ΤΕΜ",1,"LVM",1,"KWA:107161932"]
["LDX:L0002173","deep-groove ball bearing",267,"ΤΕΜ",1,"LVM",1,"LDX:L0002173"]
["LDX:L0420934-0001","Terminal board equipped",264,"ΤΕΜ",1,"LVM",1,"LDX:L04209340001"]
["LMH:101259337","*Spare part* Bearing shield DE B3 4-pole, standard paint finish 1LE0 Ah 355",1458,"ΤΕΜ",1,"LVM",1,"LMH:101259337"]
["LMH:6100380205","*Spare part* Oil seal B110*140*12 1LG0 Ah 355",75,"ΤΕΜ",1,"LVM",1,"LMH:6100380205"]
["LMH:6100604515","*Repair part* Bearing shield DE B3 1LG0 Ah 100",86,"ΤΕΜ",1,"LVM",1,"LMH:6100604515"]
["LMH:ZSD50878080040000","*Spare part* Terminal board complete 6-P-M4 1LE0 Ah 080, 090",43,"ΤΕΜ",1,"LVM",1,"LMH:ZSD50878080040000"]
["XZM:20000000300323","*Spare part* Fan 7.04 D127 PPGF30 1LA7, 1LA9 Ah 071",53,"ΤΕΜ",1,"LVM",1,"XZM:20000000300323"]
["XZM:21297031601000","*Repair part* Bearing shield B3 1.40 or 6.20 1LA7 Ah 071",42,"ΤΕΜ",1,"LVM",1,"XZM:21297031601000"]
["XZM:27000804570390","*Repair part* Enclosure foot 4.09 clockwise 1LE1 Ah 132",97,"ΤΕΜ",1,"LVM",1,"XZM:27000804570390"]
["XZM:27000812982692","*Repair part* Flange B5 1.40 1LE1 Ah 160",410,"ΤΕΜ",1,"LVM",1,"XZM:27000812982692"]
["XZM:27000915133650","*Repair part* Flange B14 1.40 FT130 1LA7, 1LA9 Ah 080",210,"ΤΕΜ",1,"LVM",1,"XZM:27000915133650"]
["XZM:50000251000025","ball bearing 6209-2RZC4",366,"ΤΕΜ",1,"LVM",1,"XZM:50000251000025"]
["XZM:50150080004000","*Repair part* Spring washer 1.58 SN60098x 73 1LE1 Ah 080-090",42,"ΤΕΜ",1,"LVM",1,"XZM:50150080004000"]
["XZM:50748160300002","*Spare part* Fan cover 7.40 Sheet metal 1LE Ah 160",87,"ΤΕΜ",1,"LVM",1,"XZM:50748160300002"]
["XZM:50848100002410","*Repair part* TB upper part 5.44 2xDM32 1LE1 Ah 100-112",42,"ΤΕΜ",1,"LVM",1,"XZM:50848100002410"]
["XZM:51177132101001","*Repair part* Bearing cover inside 1.65 6.24 1LE1 Ah 132",122,"ΤΕΜ",1,"LVM",1,"XZM:51177132101001"]
["XZM:51298090100102","bearing shield 1LE15..-0E",55,"ΤΕΜ",1,"LVM",1,"XZM:51298090100102"]
["XZM:51298180100010","*Spare part* Bearing shield B3 1.40 or 6.20 H03 Q01 1LE Ah 180",490,"ΤΕΜ",1,"LVM",1,"XZM:51298180100010"]
["XZM:55158160580001","*Repair part* Connection parts for brake BFK458-20 1LE Ah 160-180",42,"ΤΕΜ",1,"LVM",1,"XZM:55158160580001"]
["XZM:55198180071052","*Spare part* Forced ventilation F70+F01 WISTRO C=600 1LE15...-1E, Ah 180",1693,"ΤΕΜ",1,"LVM",1,"XZM:55198180071052"]
["XZM:58398100001001","Modification kit for motors 1LE1 standard version, IP55 AH100, 2-8-pole; IMB3 to IMB5 Part No. 1.1",66,"ΤΕΜ",1,"LVM",1,"XZM:58398100001001"]
["XZM:58398132008001","Modification kit for motor 1LE1 Standard version, IP55 Size 132, B5 to L22 Refit bearings for increased cross forces for IMB3/B5/B14, Part No. 36739",118,"ΤΕΜ",1,"LVM",1,"XZM:58398132008001"]
["XZM:58398160007006","Modification kit for motors 1LE1 Standard version, IP55 AH160; Installation B3 according to L22+L23 Part No. 1.7",268,"ΤΕΜ",1,"LVM",1,"XZM:58398160007006"]
["XZM:58398180013001","Modification kit for motors 1LE1 standard version, IP55 AH180; 2-8-pole; Installation of 6x PTC thermistor in winding Retrofit Q12; Part No. 1.13.1",194,"ΤΕΜ",1,"LVM",1,"XZM:58398180013001"]
["XZM:A5E33674456","bearing shield NDE 1LE10-1E",408,"ΤΕΜ",1,"LVM",1,"XZM:A5E33674456"]
["XZM:A5E44460499","Shield 1MB1.53-1E B5 machined Q01 Exd",2394,"ΤΕΜ",1,"LVM",1,"XZM:A5E44460499"]
["XZM:A5E44575081","Endshield B3 DE 1B GG25 6306 EXD L21 Exd",3325,"ΤΕΜ",1,"LVM",1,"XZM:A5E44575081"]
["XZM:A5E45843705","Shield B14 P01 1B 6306 EXD   L21 Exd",1680,"ΤΕΜ",1,"LVM",1,"XZM:A5E45843705"]
["1LE1001-1AB41-8FA4","SIMOTICS GP motor type: 1AV2104B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * frame size 100L * 2.2 kW (50 Hz) 2.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 230 VD/400 VY IM B 5, flange: FF215 (A250) without motor protection Terminal box at top",566,"ΤΕΜ",1,"LVM",1,"1LE10011AB418FA4"]
["1LE1001-1AB43-3AA6","SIMOTICS GP motor type: 1AV2104B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * frame size 100L * 2.2 kW (50 Hz) 2.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 3, without motor protection Terminal box on left-hand side",577,"ΤΕΜ",1,"LVM",1,"1LE10011AB433AA6"]
["1LE1001-1AB52-1FB6","SIMOTICS GP motor type: 1AV2105B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * frame size 100L * 3 kW (50 Hz) 3.45 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",753,"ΤΕΜ",1,"LVM",1,"1LE10011AB521FB6"]
["1LE1001-1AC40-4FB4","SIMOTICS GP motor type: 1AV2104C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * frame size 100L * 1.5 kW (50 Hz) 1.75 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",593,"ΤΕΜ",1,"LVM",1,"1LE10011AC404FB4"]
["1LE1001-1AC43-4AA6","SIMOTICS GP motor type: 1AV2104C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * frame size 100L * 1.5 kW (50 Hz) 1.75 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box on left-hand side",544,"ΤΕΜ",1,"LVM",1,"1LE10011AC434AA6"]
["1LE1001-1BA22-1JA6","SIMOTICS GP motor type: 1AV2112A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * frame size 112M, * 4 kW (50 Hz) 4.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF215 (A250) without motor protection Terminal box on left-hand side",795,"ΤΕΜ",1,"LVM",1,"1LE10011BA221JA6"]
["1LE1001-1BA24-0FA4","SIMOTICS GP motor type: 1AV2112A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * frame size 112M, * 4 kW (50 Hz) 4.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 500 VD * IM B 5, flange: FF215 (A250) without motor protection Terminal box at top",698,"ΤΕΜ",1,"LVM",1,"1LE10011BA240FA4"]
["1LE1001-1BB23-4AC4","SIMOTICS GP motor type: 1AV2112B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * frame size 112M, * 4 kW (50 Hz) 4.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",809,"ΤΕΜ",1,"LVM",1,"1LE10011BB234AC4"]
["1LE1001-1BC22-1GB5","SIMOTICS GP motor type: 1AV2112C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * frame size 112M, * 2.2 kW (50 Hz) 2.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",821,"ΤΕΜ",1,"LVM",1,"1LE10011BC221GB5"]
["1LE1001-1BC23-3AA4","SIMOTICS GP motor type: 1AV2112C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * frame size 112M, * 2.2 kW (50 Hz) 2.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 3, without motor protection Terminal box at top",649,"ΤΕΜ",1,"LVM",1,"1LE10011BC233AA4"]
["1LE1001-1CA03-3FB7","SIMOTICS GP motor type: 1AV2130A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * frame size 132S, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 5, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1074,"ΤΕΜ",1,"LVM",1,"1LE10011CA033FB7"]
["1LE1001-1CA12-1AB5","SIMOTICS GP motor type: 1AV2131A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 132S, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",1222,"ΤΕΜ",1,"LVM",1,"1LE10011CA121AB5"]
["1LE1001-1CA12-2WB7","SIMOTICS GP motor type: 1AV2131A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 132S, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 15 * Flange: FF265 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1265,"ΤΕΜ",1,"LVM",1,"1LE10011CA122WB7"]
["1LE1001-1CA64-0JA4","SIMOTICS GP motor type: 1AV2136A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure, increased power High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 132M, * 11 kW (50 Hz) 12.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 500 VD * IM B 35 * Flange: FF265 (A300) without motor protection Terminal box at top",1491,"ΤΕΜ",1,"LVM",1,"1LE10011CA640JA4"]
["1LE1001-1CB03-3FA7","SIMOTICS GP motor type: 1AV2130B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * frame size 132S, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 5, flange: FF265 (A300) without motor protection Terminal box below",1043,"ΤΕΜ",1,"LVM",1,"1LE10011CB033FA7"]
["1LE1001-1CB20-4AA7","SIMOTICS GP motor type: 1AV2132B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 132M, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box below",1169,"ΤΕΜ",1,"LVM",1,"1LE10011CB204AA7"]
["1LE1001-1CB22-1JA4","SIMOTICS GP motor type: 1AV2132B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 132M, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF265 (A300) without motor protection Terminal box at top",1219,"ΤΕΜ",1,"LVM",1,"1LE10011CB221JA4"]
["1LE1001-1CB24-0AF4","SIMOTICS GP motor type: 1AV2132B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 132M, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 500 VD * IM B 3, 1 KTY84-130 temperature sensor (2 terminals) Terminal box at top",1198,"ΤΕΜ",1,"LVM",1,"1LE10011CB240AF4"]
["1LE1001-1CC00-4WB6","SIMOTICS GP motor type: 1AV2130C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * frame size 132S, * 3 kW (50 Hz) 3.45 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF265 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1022,"ΤΕΜ",1,"LVM",1,"1LE10011CC004WB6"]
["1LE1001-1CC02-2AB6","SIMOTICS GP motor type: 1AV2130C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * frame size 132S, * 3 kW (50 Hz) 3.45 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",937,"ΤΕΜ",1,"LVM",1,"1LE10011CC022AB6"]
["1LE1001-1CC03-4JB6","SIMOTICS GP motor type: 1AV2130C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * frame size 132S, * 3 kW (50 Hz) 3.45 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1007,"ΤΕΜ",1,"LVM",1,"1LE10011CC034JB6"]
["1LE1001-1CC22-1JB7","SIMOTICS GP motor type: 1AV2132C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * frame size 132M, * 4 kW (50 Hz) 4.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1231,"ΤΕΜ",1,"LVM",1,"1LE10011CC221JB7"]
["1LE1001-1CC22-2JC6","SIMOTICS GP motor type: 1AV2132C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * frame size 132M, * 4 kW (50 Hz) 4.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",1237,"ΤΕΜ",1,"LVM",1,"1LE10011CC222JC6"]
["1LE1001-1CC24-0FA4","SIMOTICS GP motor type: 1AV2132C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * frame size 132M, * 4 kW (50 Hz) 4.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 500 VD * IM B 5, flange: FF265 (A300) without motor protection Terminal box at top",1029,"ΤΕΜ",1,"LVM",1,"1LE10011CC240FA4"]
["1LE1001-1CC32-1AA7","SIMOTICS GP motor type: 1AV2133C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * frame size 132M, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, without motor protection Terminal box below",1321,"ΤΕΜ",1,"LVM",1,"1LE10011CC321AA7"]
["1LE1001-1CC33-4AC7","SIMOTICS GP motor type: 1AV2133C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 6-pole * frame size 132M, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",1419,"ΤΕΜ",1,"LVM",1,"1LE10011CC334AC7"]
["1LE1001-1CD01-8FA4","SIMOTICS GP motor type: 1AV2130D low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency, 8-pole * frame size 132S, * 2.2 kW (50 Hz) 2.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 230 VD/400 VY IM B 5, flange: FF265 (A300) without motor protection Terminal box at top",1176,"ΤΕΜ",1,"LVM",1,"1LE10011CD018FA4"]
["1LE1001-1DA22-2AC6","SIMOTICS GP motor type: 1AV2162A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 160M, * 11 kW (50 Hz) 12.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",1630,"ΤΕΜ",1,"LVM",1,"1LE10011DA222AC6"]
["1LE1001-1DA23-3JA5","SIMOTICS GP motor type: 1AV2162A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 160M, * 11 kW (50 Hz) 12.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 35 * Flange: FF300 (A350) without motor protection Terminal box on RHS",1639,"ΤΕΜ",1,"LVM",1,"1LE10011DA233JA5"]
["1LE1001-1DA30-4FA6","SIMOTICS GP motor type: 1AV2163A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 160M, * 15 kW (50 Hz) 17.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF300 (A350) without motor protection Terminal box on left-hand side",2010,"ΤΕΜ",1,"LVM",1,"1LE10011DA304FA6"]
["1LE1001-1DA32-1AA6","SIMOTICS GP motor type: 1AV2163A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 160M, * 15 kW (50 Hz) 17.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, without motor protection Terminal box on left-hand side",1975,"ΤΕΜ",1,"LVM",1,"1LE10011DA321AA6"]
["1LE1001-1DA33-1JA4","SIMOTICS GP motor type: 1AV2163A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 160M, * 15 kW (50 Hz) 17.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60Hz 400VD/690VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2005,"ΤΕΜ",1,"LVM",1,"1LE10011DA331JA4"]
["1LE1001-1DA42-1AB6","SIMOTICS GP motor type: 1AV2164A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 160L, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",2425,"ΤΕΜ",1,"LVM",1,"1LE10011DA421AB6"]
["1LE1001-1DA43-3FB4","SIMOTICS GP motor type: 1AV2164A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 160L, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2444,"ΤΕΜ",1,"LVM",1,"1LE10011DA433FB4"]
["1LE1001-1DA43-4GC7","SIMOTICS GP motor type: 1AV2164A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 160L, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",2508,"ΤΕΜ",1,"LVM",1,"1LE10011DA434GC7"]
["1LE1001-1DB22-1JB6","SIMOTICS GP motor type: 1AV2162B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 160M, * 11 kW (50 Hz) 12.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1768,"ΤΕΜ",1,"LVM",1,"1LE10011DB221JB6"]
["1LE1001-1DB22-3JA4","SIMOTICS GP motor type: 1AV2162B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 160M, * 11 kW (50 Hz) 12.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 240 VD/415 VY 3 AC 60 Hz 480 VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",1607,"ΤΕΜ",1,"LVM",1,"1LE10011DB223JA4"]
["1LE1001-1DB40-4AB4","SIMOTICS GP motor type: 1AV2164B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 160L, * 15 kW (50 Hz) 17.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1968,"ΤΕΜ",1,"LVM",1,"1LE10011DB404AB4"]
["1LE1001-1DB43-3GA4","SIMOTICS GP motor type: 1AV2164B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 160L, * 15 kW (50 Hz) 17.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF300 (A350) without motor protection Terminal box at top",2016,"ΤΕΜ",1,"LVM",1,"1LE10011DB433GA4"]
["1LE1001-1DB61-7JA4","SIMOTICS GP motor type: 1AV2166B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure, increased power High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 160L, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 220 VD/380 VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2366,"ΤΕΜ",1,"LVM",1,"1LE10011DB617JA4"]
["1LE1001-1DB63-5JA4","SIMOTICS GP motor type: 1AV2166B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure, increased power High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 160L, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2366,"ΤΕΜ",1,"LVM",1,"1LE10011DB635JA4"]
["1LE1001-1DC22-2GC5","SIMOTICS GP motor type: 1AV2162C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 6-pole * frame size 160M, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",1826,"ΤΕΜ",1,"LVM",1,"1LE10011DC222GC5"]
["1LE1001-1DC42-1FB7","SIMOTICS GP motor type: 1AV2164C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 6-pole * frame size 160L, * 11 kW (50 Hz) 12.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",2414,"ΤΕΜ",1,"LVM",1,"1LE10011DC421FB7"]
["1LE1001-1DC42-7DB4","SIMOTICS GP motor type: 1AV2164C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 6-pole * frame size 160L, * 11 kW (50 Hz) 12.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 500VY * 3 AC 60Hz 575VY IM V 6, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2205,"ΤΕΜ",1,"LVM",1,"1LE10011DC427DB4"]
["1LE1001-1DC43-4FA7","SIMOTICS GP motor type: 1AV2164C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 6-pole * frame size 160L, * 11 kW (50 Hz) 12.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF300 (A350) without motor protection Terminal box below",2268,"ΤΕΜ",1,"LVM",1,"1LE10011DC434FA7"]
["1LE1001-1DD23-4AA4","SIMOTICS GP motor type: 1AV2162D low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency, 8-pole * frame size 160M, * 4 kW (50 Hz) 4.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box at top",1591,"ΤΕΜ",1,"LVM",1,"1LE10011DD234AA4"]
["1LE1001-1EA26-3JA4","SIMOTICS GP motor type: 1AV2182A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 180 * 22 kW (50 Hz) 24.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 230 VDD * 50 Hz 460 VD * 12 main terminals electrical according to NEMA IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2786,"ΤΕΜ",1,"LVM",1,"1LE10011EA263JA4"]
["1LE1001-1EA66-1FA4","SIMOTICS GP motor type: 1AV2186A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure, increased power High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 180 * 30 kW (50 Hz) 33.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 230 VYY * 60 Hz 460 VY * 9 main terminals electrical according to NEMA IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",3512,"ΤΕΜ",1,"LVM",1,"1LE10011EA661FA4"]
["1LE1001-1EB43-1FA4","SIMOTICS GP motor type: 1AV2184B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 180 * 22 kW (50 Hz) 25.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60Hz 400VD/690VY IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",2725,"ΤΕΜ",1,"LVM",1,"1LE10011EB431FA4"]
["1LE1001-1EC66-1JA4","SIMOTICS GP motor type: 1AV2186C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure, increased power High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 6-pole * frame size 180 * 18.5 kW (50 Hz) 22 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 230 VYY * 60 Hz 460 VY * 9 main terminals electrical according to NEMA IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",3510,"ΤΕΜ",1,"LVM",1,"1LE10011EC661JA4"]
["1LE1001-2AA43-1JA4","SIMOTICS GP motor type: 1AV2204A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 200 * 30 kW (50 Hz) 33.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60Hz 400VD/690VY IM B 35 * Flange: FF350 (A400) without motor protection Terminal box at top",3591,"ΤΕΜ",1,"LVM",1,"1LE10012AA431JA4"]
["1LE1001-2AA52-2JA4","SIMOTICS GP motor type: 1AV2205A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 200 * 37 kW (50 Hz) 41.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF350 (A400) without motor protection Terminal box at top",4368,"ΤΕΜ",1,"LVM",1,"1LE10012AA522JA4"]
["1LE1001-2AA66-1JA4","SIMOTICS GP motor type: 1AV2206A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure, increased power High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 200 * 45 kW (50 Hz) 51 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 230 VYY * 60 Hz 460 VY * 9 main terminals electrical according to NEMA IM B 35 * Flange: FF350 (A400) without motor protection Terminal box at top",5248,"ΤΕΜ",1,"LVM",1,"1LE10012AA661JA4"]
["1LE1001-2AC50-4AA4","SIMOTICS GP motor type: 1AV2205C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, 60 Hz, P60: IE1 in EEA: minimum efficiency according to applicable statutory regulations to be considered 6-pole * frame size 200 * 22 kW (50 Hz) 26.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box at top",3800,"ΤΕΜ",1,"LVM",1,"1LE10012AC504AA4"]
["1LE1001-2AC61-8AA4","SIMOTICS GP motor type: 1AV2206C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure, increased power High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 6-pole * frame size 200 * 30 kW (50 Hz) 34.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 230 VD/400 VY IM B 3, without motor protection Terminal box at top",5170,"ΤΕΜ",1,"LVM",1,"1LE10012AC618AA4"]
["1LE1001-2AD53-5AA4","SIMOTICS GP motor type: 1AV2205D low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, 8-pole * frame size 200 * 15 kW (50 Hz) 18 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 3, without motor protection Terminal box at top",3841,"ΤΕΜ",1,"LVM",1,"1LE10012AD535AA4"]
["1LE1003-0DA23-4AB6","SIMOTICS GP motor type: 1AV3082A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 2-pole * frame size 80M * 0.75 kW (50 Hz) 0.86 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, MOTOR PROTECTION WITH 1 PTC THERMISTORS FOR SHUTDOWN Terminal box lateral left",365,"ΤΕΜ",1,"LVM",1,"1LE10030DA234AB6"]
["1LE1003-0DA30-4FB5","SIMOTICS GP motor type: 1AV3083A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 2-pole * frame size 80M * 1.1 kW (50 Hz) 1.27 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF165 (A200) MOTOR PROTECTION WITH 1 PTC THERMISTORS FOR SHUTDOWN Terminal box lateral right",441,"ΤΕΜ",1,"LVM",1,"1LE10030DA304FB5"]
["1LE1003-0DA33-4FA5","SIMOTICS GP motor type: 1AV3083A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 2-pole * frame size 80M * 1.1 kW (50 Hz) 1.27 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF165 (A200) WITHOUT MOTOR PROTECTION Terminal box lateral right",420,"ΤΕΜ",1,"LVM",1,"1LE10030DA334FA5"]
["1LE1003-0DB23-3GB6","SIMOTICS GP motor type: 1AV3082B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency, 4-pole * frame size 80M * 0.55 kW (50 Hz) 0.63 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF165 (A200) MOTOR PROTECTION WITH 1 PTC THERMISTORS FOR SHUTDOWN Terminal box lateral left",409,"ΤΕΜ",1,"LVM",1,"1LE10030DB233GB6"]
["1LE1003-0DB32-1JB5","SIMOTICS GP motor type: 1AV3083B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 4-pole * frame size 80M * 0.75 kW (50 Hz) 0.86 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF165 (A200) MOTOR PROTECTION WITH 1 PTC THERMISTORS FOR SHUTDOWN Terminal box lateral right",441,"ΤΕΜ",1,"LVM",1,"1LE10030DB321JB5"]
["1LE1003-0DB33-1JA4","SIMOTICS GP motor type: 1AV3083B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 4-pole * frame size 80M * 0.75 kW (50 Hz) 0.86 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60Hz 400VD/690VY IM B 35 * Flange: FF165 (A200) WITHOUT MOTOR PROTECTION Terminal box at top",401,"ΤΕΜ",1,"LVM",1,"1LE10030DB331JA4"]
["1LE1003-0DC22-1GA6","SIMOTICS GP motor type: 1AV3082C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency, 6-pole * frame size 80M * 0.37 kW (50 Hz) 0.43 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF165 (A200) without motor protection Terminal box lateral left",379,"ΤΕΜ",1,"LVM",1,"1LE10030DC221GA6"]
["1LE1003-0DC32-2GA6","SIMOTICS GP motor type: 1AV3083C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency, 6-pole * frame size 80M * 0.55 kW (50 Hz) 0.63 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF165 (A200) without motor protection Terminal box lateral left",409,"ΤΕΜ",1,"LVM",1,"1LE10030DC322GA6"]
["1LE1003-0EA02-1AB4","SIMOTICS GP motor type: 1AV3090A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 2-pole * frame size 90S * 1.5 kW (50 Hz) 1.75 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, MOTOR PROTECTION WITH 1 PTC THERMISTORS FOR SHUTDOWN Terminal box at top",475,"ΤΕΜ",1,"LVM",1,"1LE10030EA021AB4"]
["1LE1003-0EA03-4AB5","SIMOTICS GP motor type: 1AV3090A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 2-pole * frame size 90S * 1.5 kW (50 Hz) 1.75 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, MOTOR PROTECTION WITH 1 PTC THERMISTORS FOR SHUTDOWN Terminal box lateral right",474,"ΤΕΜ",1,"LVM",1,"1LE10030EA034AB5"]
["1LE1003-0EA42-2AC4","SIMOTICS GP motor type: 1AV3094A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 2-pole * frame size 90L * 2.2 kW (50 Hz) 2.55 kW (60 Hz) 60 Hz, P60: IE2 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 2 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",644,"ΤΕΜ",1,"LVM",1,"1LE10030EA422AC4"]
["1LE1003-0EB00-4JB5","SIMOTICS GP motor type: 1AV3090B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 4-pole * frame size 90S * 1.1 kW (50 Hz) 1.27 kW (60 Hz) 60 Hz, P60: IE2 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF165 (A200) MOTOR PROTECTION WITH 1 PTC THERMISTORS FOR SHUTDOWN Terminal box lateral right",496,"ΤΕΜ",1,"LVM",1,"1LE10030EB004JB5"]
["1LE1003-0EB40-4AA4","SIMOTICS GP motor type: 1AV3094B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 4-pole * frame size 90L * 1.5 kW (50 Hz) 1.75 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, WITHOUT MOTOR PROTECTION Terminal box at top",495,"ΤΕΜ",1,"LVM",1,"1LE10030EB404AA4"]
["1LE1003-0EB42-2AB5","SIMOTICS GP motor type: 1AV3094B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 4-pole * frame size 90L * 1.5 kW (50 Hz) 1.75 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, MOTOR PROTECTION WITH 1 PTC THERMISTORS FOR SHUTDOWN Terminal box lateral right",537,"ΤΕΜ",1,"LVM",1,"1LE10030EB422AB5"]
["1LE1003-0EC03-1FA4","SIMOTICS GP motor type: 1AV3090C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 90S * 0.75 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60Hz 400VD/690VY IM B 5, flange: FF165 (A200) without motor protection Terminal box at top",465,"ΤΕΜ",1,"LVM",1,"1LE10030EC031FA4"]
["1LE1003-0EC42-1FA4","SIMOTICS GP motor type: 1AV3094C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 90L * 1.1 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF165 (A200) without motor protection Terminal box at top",563,"ΤΕΜ",1,"LVM",1,"1LE10030EC421FA4"]
["1LE1003-0EC43-3AA4","SIMOTICS GP motor type: 1AV3094C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 90L * 1.1 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 3, without motor protection Terminal box at top",529,"ΤΕΜ",1,"LVM",1,"1LE10030EC433AA4"]
["1LE1003-1AA42-2AC4","SIMOTICS GP motor type: 1AV3104A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * frame size 100L * 3 kW (50 Hz) 3.45 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",716,"ΤΕΜ",1,"LVM",1,"1LE10031AA422AC4"]
["1LE1003-1AA43-4JC7","SIMOTICS GP motor type: 1AV3104A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * frame size 100L * 3 kW (50 Hz) 3.45 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF215 (A250) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",815,"ΤΕΜ",1,"LVM",1,"1LE10031AA434JC7"]
["1LE1003-1AB42-2FB6","SIMOTICS GP motor type: 1AV3104B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 100L * 2.2 kW (50 Hz) 2.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",715,"ΤΕΜ",1,"LVM",1,"1LE10031AB422FB6"]
["1LE1003-1AB43-4FC7","SIMOTICS GP motor type: 1AV3104B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 100L * 2.2 kW (50 Hz) 2.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF215 (A250) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",760,"ΤΕΜ",1,"LVM",1,"1LE10031AB434FC7"]
["1LE1003-1AB52-2FA5","SIMOTICS GP motor type: 1AV3105B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 4-pole * frame size 100L * 3 kW (50 Hz) 3.45 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF215 (A250) Without motor protection Terminal box on RHS",742,"ΤΕΜ",1,"LVM",1,"1LE10031AB522FA5"]
["1LE1003-1AC40-4FA6","SIMOTICS GP motor type: 1AV3104C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 100L * 1.5 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF215 (A250) without motor protection Terminal box on left-hand side",649,"ΤΕΜ",1,"LVM",1,"1LE10031AC404FA6"]
["1LE1003-1AC42-2JC4","SIMOTICS GP motor type: 1AV3104C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 100L * 1.5 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF215 (A250) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",705,"ΤΕΜ",1,"LVM",1,"1LE10031AC422JC4"]
["1LE1003-1AC43-4AB6","SIMOTICS GP motor type: 1AV3104C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 100L * 1.5 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",668,"ΤΕΜ",1,"LVM",1,"1LE10031AC434AB6"]
["1LE1003-1BA23-4FC6","SIMOTICS GP motor type: 1AV3112A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * frame size 112M, * 4 kW (50 Hz) 4.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF215 (A250) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",940,"ΤΕΜ",1,"LVM",1,"1LE10031BA234FC6"]
["1LE1003-1BB20-4JB6","SIMOTICS GP motor type: 1AV3112B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 4-pole * frame size 112M, * 4 kW (50 Hz) 4.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",962,"ΤΕΜ",1,"LVM",1,"1LE10031BB204JB6"]
["1LE1003-1BB23-4GA4","SIMOTICS GP motor type: 1AV3112B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 4-pole * frame size 112M, * 4 kW (50 Hz) 4.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF215 (A250) Without motor protection Terminal box at top",837,"ΤΕΜ",1,"LVM",1,"1LE10031BB234GA4"]
["1LE1003-1BC20-4FB7","SIMOTICS GP motor type: 1AV3112C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 112M, * 2.2 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",875,"ΤΕΜ",1,"LVM",1,"1LE10031BC204FB7"]
["1LE1003-1BC23-4GA5","SIMOTICS GP motor type: 1AV3112C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 112M, * 2.2 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF215 (A250) without motor protection Terminal box on RHS",813,"ΤΕΜ",1,"LVM",1,"1LE10031BC234GA5"]
["1LE1003-1CA02-1FB7","SIMOTICS GP motor type: 1AV3130A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 2-pole * frame size 132S, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1172,"ΤΕΜ",1,"LVM",1,"1LE10031CA021FB7"]
["1LE1003-1CA03-3JA6","SIMOTICS GP motor type: 1AV3130A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 2-pole * frame size 132S, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 35, flange: FF265 (A300) Without motor protection Terminal box on left-hand side",1082,"ΤΕΜ",1,"LVM",1,"1LE10031CA033JA6"]
["1LE1003-1CA12-1WB7","SIMOTICS GP motor type: 1AV3131A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 2-pole * frame size 132S, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 15 * Flange: FF265 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1437,"ΤΕΜ",1,"LVM",1,"1LE10031CA121WB7"]
["1LE1003-1CA13-3JB6","SIMOTICS GP motor type: 1AV3131A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 2-pole * frame size 132S, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 35, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1422,"ΤΕΜ",1,"LVM",1,"1LE10031CA133JB6"]
["1LE1003-1CA13-5JA4","SIMOTICS GP motor type: 1AV3131A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 2-pole * frame size 132S, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 35, flange: FF265 (A300) Without motor protection Terminal box at top",1266,"ΤΕΜ",1,"LVM",1,"1LE10031CA135JA4"]
["1LE1003-1CB03-3JA4","SIMOTICS GP motor type: 1AV3130B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 132S, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 35, flange: FF265 (A300) Without motor protection Terminal box at top",1101,"ΤΕΜ",1,"LVM",1,"1LE10031CB033JA4"]
["1LE1003-1CB21-7JA4","SIMOTICS GP motor type: 1AV3132B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 132M, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 220 VD/380 VY IM B 35, flange: FF265 (A300) Without motor protection Terminal box at top",1364,"ΤΕΜ",1,"LVM",1,"1LE10031CB217JA4"]
["1LE1003-1CB23-3FB4","SIMOTICS GP motor type: 1AV3132B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 132M, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 5, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1454,"ΤΕΜ",1,"LVM",1,"1LE10031CB233FB4"]
["1LE1003-1CB23-4JA5","SIMOTICS GP motor type: 1AV3132B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 132M, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35, flange: FF265 (A300) Without motor protection Terminal box on RHS",1384,"ΤΕΜ",1,"LVM",1,"1LE10031CB234JA5"]
["1LE1003-1CC02-2GB6","SIMOTICS GP motor type: 1AV3130C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 132S, * 3 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1098,"ΤΕΜ",1,"LVM",1,"1LE10031CC022GB6"]
["1LE1003-1CC03-3GB7","SIMOTICS GP motor type: 1AV3130C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 132S, * 3 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1141,"ΤΕΜ",1,"LVM",1,"1LE10031CC033GB7"]
["1LE1003-1CC20-2AA4","SIMOTICS GP motor type: 1AV3132C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 132M, * 4 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B3 without motor protection Terminal box at top",1080,"ΤΕΜ",1,"LVM",1,"1LE10031CC202AA4"]
["1LE1003-1CC23-4GB4","SIMOTICS GP motor type: 1AV3132C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 132M, * 4 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1241,"ΤΕΜ",1,"LVM",1,"1LE10031CC234GB4"]
["1LE1003-1CC32-1JA6","SIMOTICS GP motor type: 1AV3133C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 132M, * 5.5 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF265 (A300) without motor protection Terminal box on left-hand side",1536,"ΤΕΜ",1,"LVM",1,"1LE10031CC321JA6"]
["1LE1003-1CC33-4FA5","SIMOTICS GP motor type: 1AV3133C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 132M, * 5.5 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF265 (A300) without motor protection Terminal box on RHS",1490,"ΤΕΜ",1,"LVM",1,"1LE10031CC334FA5"]
["1LE1003-1CC33-4WC6","SIMOTICS GP motor type: 1AV3133C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 132M, * 5.5 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF265 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",1649,"ΤΕΜ",1,"LVM",1,"1LE10031CC334WC6"]
["1LE1003-1CD22-1GB7","SIMOTICS GP motor type: 1AV3132D low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 8-pole * frame size 132M, * 3 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1884,"ΤΕΜ",1,"LVM",1,"1LE10031CD221GB7"]
["1LE1003-1CD23-4GC5","SIMOTICS GP motor type: 1AV3132D low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 8-pole * frame size 132M, * 3 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",1890,"ΤΕΜ",1,"LVM",1,"1LE10031CD234GC5"]
["1LE1003-1DA20-4WB6","SIMOTICS GP motor type: 1AV3162A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 2-pole * frame size 160M, * 11 kW (50 Hz) 12.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF300 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1886,"ΤΕΜ",1,"LVM",1,"1LE10031DA204WB6"]
["1LE1003-1DA23-0AA4","SIMOTICS GP motor type: 1AV3162A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 2-pole * frame size 160M, * 11 kW (50 Hz) 12.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 380 VD/660 VY IM B3 Without motor protection Terminal box at top",1654,"ΤΕΜ",1,"LVM",1,"1LE10031DA230AA4"]
["1LE1003-1DA32-2AB7","SIMOTICS GP motor type: 1AV3163A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 2-pole * frame size 160M, * 15 kW (50 Hz) 17.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box below",2258,"ΤΕΜ",1,"LVM",1,"1LE10031DA322AB7"]
["1LE1003-1DA33-3AB6","SIMOTICS GP motor type: 1AV3163A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 2-pole * frame size 160M, * 15 kW (50 Hz) 17.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",2311,"ΤΕΜ",1,"LVM",1,"1LE10031DA333AB6"]
["1LE1003-1DA42-7AA4","SIMOTICS GP motor type: 1AV3164A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 2-pole * frame size 160L, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 500VY * 3 AC 60Hz 575VY IM B3 Without motor protection Terminal box at top",2494,"ΤΕΜ",1,"LVM",1,"1LE10031DA427AA4"]
["1LE1003-1DA44-0FA4","SIMOTICS GP motor type: 1AV3164A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 2-pole * frame size 160L, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 500 VD * IM B 5, flange: FF300 (A350) Without motor protection Terminal box at top",2582,"ΤΕΜ",1,"LVM",1,"1LE10031DA440FA4"]
["1LE1003-1DB22-1JB6","SIMOTICS GP motor type: 1AV3162B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 4-pole * frame size 160M, * 11 kW (50 Hz) 12.6 kW (60 Hz) 60 Hz, P60: IE2 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1949,"ΤΕΜ",1,"LVM",1,"1LE10031DB221JB6"]
["1LE1003-1DB22-2JB7","SIMOTICS GP motor type: 1AV3162B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 4-pole * frame size 160M, * 11 kW (50 Hz) 12.6 kW (60 Hz) 60 Hz, P60: IE2 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1896,"ΤΕΜ",1,"LVM",1,"1LE10031DB222JB7"]
["1LE1003-1DB23-4JC4","SIMOTICS GP motor type: 1AV3162B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 4-pole * frame size 160M, * 11 kW (50 Hz) 12.6 kW (60 Hz) 60 Hz, P60: IE2 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",1876,"ΤΕΜ",1,"LVM",1,"1LE10031DB234JC4"]
["1LE1003-1DB43-4JB7","SIMOTICS GP motor type: 1AV3164B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 4-pole * frame size 160L, * 15 kW (50 Hz) 17.3 kW (60 Hz) 60 Hz, P60: IE2 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",2386,"ΤΕΜ",1,"LVM",1,"1LE10031DB434JB7"]
["1LE1003-1DC20-4GB6","SIMOTICS GP motor type: 1AV3162C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 160M, * 7.5 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1974,"ΤΕΜ",1,"LVM",1,"1LE10031DC204GB6"]
["1LE1003-1DC22-2FC4","SIMOTICS GP motor type: 1AV3162C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 160M, * 7.5 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",1954,"ΤΕΜ",1,"LVM",1,"1LE10031DC222FC4"]
["1LE1003-1DC41-8FA4","SIMOTICS GP motor type: 1AV3164C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 160L, * 11 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 230 VD/400 VY IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",2517,"ΤΕΜ",1,"LVM",1,"1LE10031DC418FA4"]
["1LE1003-1DC42-2GB7","SIMOTICS GP motor type: 1AV3164C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 160L, * 11 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",2624,"ΤΕΜ",1,"LVM",1,"1LE10031DC422GB7"]
["1LE1003-1DD20-4AB5","SIMOTICS GP motor type: 1AV3162D low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 8-pole * frame size 160M, * 4 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",2155,"ΤΕΜ",1,"LVM",1,"1LE10031DD204AB5"]
["1LE1003-1DD30-4JA5","SIMOTICS GP motor type: 1AV3163D low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 8-pole * frame size 160M, * 5.5 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF300 (A350) without motor protection Terminal box on RHS",2567,"ΤΕΜ",1,"LVM",1,"1LE10031DD304JA5"]
["1LE1003-1DD33-4GA5","SIMOTICS GP motor type: 1AV3163D low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 8-pole * frame size 160M, * 5.5 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) without motor protection Terminal box on RHS",2557,"ΤΕΜ",1,"LVM",1,"1LE10031DD334GA5"]
["1LE1003-1DD42-1JB4","SIMOTICS GP motor type: 1AV3164D low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 8-pole * frame size 160L, * 7.5 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",3099,"ΤΕΜ",1,"LVM",1,"1LE10031DD421JB4"]
["1LE1003-1DD43-3GA5","SIMOTICS GP motor type: 1AV3164D low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 8-pole * frame size 160L, * 7.5 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF300 (A350) without motor protection Terminal box on RHS",3065,"ΤΕΜ",1,"LVM",1,"1LE10031DD433GA5"]
["1LE1003-1EA62-1FA4","SIMOTICS GP motor type: 1AV3186A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure, increased power Premium Efficiency IE3, 2-pole * frame size 180 * 30 kW (50 Hz) 33.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",4044,"ΤΕΜ",1,"LVM",1,"1LE10031EA621FA4"]
["1LE1003-1EB22-2AB6","SIMOTICS GP motor type: 1AV3182B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 4-pole * frame size 180 * 18.5 kW (50 Hz) 21.3 kW (60 Hz) 60 Hz, P60: IE2 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",2578,"ΤΕΜ",1,"LVM",1,"1LE10031EB222AB6"]
["1LE1003-1EB23-5JA4","SIMOTICS GP motor type: 1AV3182B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 4-pole * frame size 180 * 18.5 kW (50 Hz) 21.3 kW (60 Hz) 60 Hz, P60: IE2 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2624,"ΤΕΜ",1,"LVM",1,"1LE10031EB235JA4"]
["1LE1003-1EB43-3AB4","SIMOTICS GP motor type: 1AV3184B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 4-pole * frame size 180 * 22 kW (50 Hz) 25.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2924,"ΤΕΜ",1,"LVM",1,"1LE10031EB433AB4"]
["1LE1003-1EC42-1AB5","SIMOTICS GP motor type: 1AV3184C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 180 * 15 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",3255,"ΤΕΜ",1,"LVM",1,"1LE10031EC421AB5"]
["1LE1003-1EC63-4FA4","SIMOTICS GP motor type: 1AV3186C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure, increased power Premium Efficiency IE3, 6-pole * frame size 180 * 18.5 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",3933,"ΤΕΜ",1,"LVM",1,"1LE10031EC634FA4"]
["1LE1003-1ED42-2JB4","SIMOTICS GP motor type: 1AV3184D low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 8-pole * frame size 180 * 11 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",3786,"ΤΕΜ",1,"LVM",1,"1LE10031ED422JB4"]
["1LE1003-2AA42-1GB6","SIMOTICS GP motor type: 1AV3204A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 2-pole * frame size 200 * 30 kW (50 Hz) 33.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",4128,"ΤΕΜ",1,"LVM",1,"1LE10032AA421GB6"]
["1LE1003-2AA63-1AA4","SIMOTICS GP motor type: 1AV3206A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure, increased power Premium Efficiency IE3, 2-pole * frame size 200 * 45 kW (50 Hz) 51 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60Hz 400VD/690VY IM B 3, without motor protection Terminal box at top",5655,"ΤΕΜ",1,"LVM",1,"1LE10032AA631AA4"]
["1LE1003-2AB52-2AC5","SIMOTICS GP motor type: 1AV3205B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 200 * 30 kW (50 Hz) 34.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",3930,"ΤΕΜ",1,"LVM",1,"1LE10032AB522AC5"]
["1LE1003-2AB64-0JA4","SIMOTICS GP motor type: 1AV3206B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure, increased power Premium Efficiency IE3, 4-pole * frame size 200 * 37 kW (50 Hz) 42.5 kW (60 Hz) 60 Hz, P60: IE2 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 500 VD * IM B 35 * Flange: FF350 (A400) without motor protection Terminal box at top",4690,"ΤΕΜ",1,"LVM",1,"1LE10032AB640JA4"]
["1LE1003-2AC56-3JA4","SIMOTICS GP motor type: 1AV3205C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 200 * 22 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 230 VDD * 50 Hz 460 VD * 12 main terminals electrical according to NEMA IM B 35 * Flange: FF350 (A400) without motor protection Terminal box at top",4492,"ΤΕΜ",1,"LVM",1,"1LE10032AC563JA4"]
["1LE1003-2AD53-3JA4","SIMOTICS GP motor type: 1AV3205D low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 8-pole * frame size 200 * 15 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 35 * Flange: FF350 (A400) without motor protection Terminal box at top",4878,"ΤΕΜ",1,"LVM",1,"1LE10032AD533JA4"]
["1LE1004-1AA42-2JB6","SIMOTICS GP motor type: 1AV4104A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 2-pole * frame size 100L * 3 kW (50 Hz) 3.45 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",900,"ΤΕΜ",1,"LVM",1,"1LE10041AA422JB6"]
["1LE1004-1AB43-3FA6","SIMOTICS GP motor type: 1AV4104B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 4-pole * frame size 100L * 2.2 kW (50 Hz) 2.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 5, flange: FF215 (A250) without motor protection Terminal box on left-hand side",806,"ΤΕΜ",1,"LVM",1,"1LE10041AB433FA6"]
["1LE1004-1AB54-0AA4","SIMOTICS GP motor type: 1AV4105B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 4-pole * frame size 100L * 3 kW (50 Hz) 3.45 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 500 VD * IM B 3, without motor protection Terminal box at top",780,"ΤΕΜ",1,"LVM",1,"1LE10041AB540AA4"]
["1LE1004-1BA23-4FB7","SIMOTICS GP motor type: 1AV4112A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 2-pole * frame size 112M, * 4 kW (50 Hz) 4.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1045,"ΤΕΜ",1,"LVM",1,"1LE10041BA234FB7"]
["1LE1004-1BB22-2GA7","SIMOTICS GP motor type: 1AV4112B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 4-pole * frame size 112M, * 4 kW (50 Hz) 4.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF215 (A250) without motor protection Terminal box below",1066,"ΤΕΜ",1,"LVM",1,"1LE10041BB222GA7"]
["1LE1004-1CA03-4JC6","SIMOTICS GP motor type: 1AV4130A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 2-pole * frame size 132S, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",1376,"ΤΕΜ",1,"LVM",1,"1LE10041CA034JC6"]
["1LE1004-1CA12-1WB5","SIMOTICS GP motor type: 1AV4131A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 2-pole * frame size 132S, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 15 * Flange: FF265 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",1680,"ΤΕΜ",1,"LVM",1,"1LE10041CA121WB5"]
["1LE1004-1CA13-4JB7","SIMOTICS GP motor type: 1AV4131A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 2-pole * frame size 132S, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1622,"ΤΕΜ",1,"LVM",1,"1LE10041CA134JB7"]
["1LE1004-1CB03-4WC7","SIMOTICS GP motor type: 1AV4130B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 4-pole * frame size 132S, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF265 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",1484,"ΤΕΜ",1,"LVM",1,"1LE10041CB034WC7"]
["1LE1004-1CB23-4JC7","SIMOTICS GP motor type: 1AV4132B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 4-pole * frame size 132M, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",1784,"ΤΕΜ",1,"LVM",1,"1LE10041CB234JC7"]
["1LE1004-1DA23-3FB7","SIMOTICS GP motor type: 1AV4162A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 2-pole * frame size 160M, * 11 kW (50 Hz) 12.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",2244,"ΤΕΜ",1,"LVM",1,"1LE10041DA233FB7"]
["1LE1004-1DA32-2AB4","SIMOTICS GP motor type: 1AV4163A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 2-pole * frame size 160M, * 15 kW (50 Hz) 17.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2623,"ΤΕΜ",1,"LVM",1,"1LE10041DA322AB4"]
["1LE1004-1DA43-3AB6","SIMOTICS GP motor type: 1AV4164A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 2-pole * frame size 160L, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",3235,"ΤΕΜ",1,"LVM",1,"1LE10041DA433AB6"]
["1LE1004-1DB22-2AB6","SIMOTICS GP motor type: 1AV4162B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 4-pole * frame size 160M, * 11 kW (50 Hz) 12.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",2144,"ΤΕΜ",1,"LVM",1,"1LE10041DB222AB6"]
["1LE1004-1DB23-4FC6","SIMOTICS GP motor type: 1AV4162B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 4-pole * frame size 160M, * 11 kW (50 Hz) 12.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",2281,"ΤΕΜ",1,"LVM",1,"1LE10041DB234FC6"]
["1LE1004-1EA22-2JA4","SIMOTICS GP motor type: 1AV4182A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4 2-pole * frame size 180M, * 22 kW (50 Hz) 24.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",3609,"ΤΕΜ",1,"LVM",1,"1LE10041EA222JA4"]
["1LE1004-1EB26-0JA4","SIMOTICS GP motor type: 1AV4182B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4 4-pole * frame size 180M, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 230 VYY * 50 Hz 460 VY * 9 main terminals electrical according to NEMA IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",3124,"ΤΕΜ",1,"LVM",1,"1LE10041EB260JA4"]
["1LE1004-1EB44-0AA4","SIMOTICS GP motor type: 1AV4184B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 4-pole * frame size 180L, * 22 kW (50 Hz) 25.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 500 VD * IM B 3, without motor protection Terminal box at top",3331,"ΤΕΜ",1,"LVM",1,"1LE10041EB440AA4"]
["1LE1004-2AB53-3AA4","SIMOTICS GP motor type: 1AV4205B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 4-pole * frame size 200L* 30 kW (50 Hz) 34.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 3, without motor protection Terminal box at top",4383,"ΤΕΜ",1,"LVM",1,"1LE10042AB533AA4"]
["1LE1501-1AB40-2FA4","SIMOTICS SD motor type: 1CV2104B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) High Efficiency IE2, 4-pole * frame size 100L * 2.2 kW (50 Hz) 2.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF215 (A250) without motor protection Terminal box at top",580,"ΤΕΜ",1,"LVM",1,"1LE15011AB402FA4"]
["1LE1501-1AB51-7JA4","SIMOTICS SD motor type: 1CV2105B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) High Efficiency IE2, 4-pole * frame size 100L * 3 kW (50 Hz) 3.45 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 220 VD/380 VY IM B 35 * Flange: FF215 (A250) without motor protection Terminal box at top",689,"ΤΕΜ",1,"LVM",1,"1LE15011AB517JA4"]
["1LE1501-1AC43-5JA4","SIMOTICS SD motor type: 1CV2104C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) High Efficiency IE2, 6-pole * frame size 100L * 1.5 kW (50 Hz) 1.75 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 35 * Flange: FF215 (A250) without motor protection Terminal box at top",606,"ΤΕΜ",1,"LVM",1,"1LE15011AC435JA4"]
["1LE1501-1CA03-1JA4","SIMOTICS SD motor type: 1CV2130A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) High Efficiency IE2, 2-pole * frame size 132S, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60Hz 400VD/690VY IM B 35 * Flange: FF265 (A300) without motor protection Terminal box at top",987,"ΤΕΜ",1,"LVM",1,"1LE15011CA031JA4"]
["1LE1501-1CA13-4JC5","SIMOTICS SD motor type: 1CV2131A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 132S, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",1393,"ΤΕΜ",1,"LVM",1,"1LE15011CA134JC5"]
["1LE1501-1CB22-7JA4","SIMOTICS SD motor type: 1CV2132B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 132M, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 500 VY 3 AC 60Hz 575VY IM B 35 * Flange: FF265 (A300) without motor protection Terminal box at top",1279,"ΤΕΜ",1,"LVM",1,"1LE15011CB227JA4"]
["1LE1501-1CB24-0AA4","SIMOTICS SD motor type: 1CV2132B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 132M, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 500 VD 3 AC 60 Hz 575 VD IM B 3, without motor protection Terminal box at top",1209,"ΤΕΜ",1,"LVM",1,"1LE15011CB240AA4"]
["1LE1501-1CD01-7JA4","SIMOTICS SD motor type: 1CV2130D low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, 8-pole * frame size 132S, * 2.2 kW (50 Hz) 2.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 220 VD/380 VY IM B 35 * Flange: FF265 (A300) without motor protection Terminal box at top",1261,"ΤΕΜ",1,"LVM",1,"1LE15011CD017JA4"]
["1LE1501-1CD22-2FA4","SIMOTICS SD motor type: 1CV2132D low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, 60 Hz, P60: IE1 8-pole * frame size 132M, * 3 kW (50 Hz) 3.45 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF265 (A300) without motor protection Terminal box at top",1474,"ΤΕΜ",1,"LVM",1,"1LE15011CD222FA4"]
["1LE1501-1DA41-7AA4","SIMOTICS SD motor type: 1CV2164A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 160L, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 220 VD/380 VY IM B 3, without motor protection Terminal box at top",2450,"ΤΕΜ",1,"LVM",1,"1LE15011DA417AA4"]
["1LE1501-1DA43-4FA4","SIMOTICS SD motor type: 1CV2164A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 160L, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",2485,"ΤΕΜ",1,"LVM",1,"1LE15011DA434FA4"]
["1LE1501-1DB61-7AA4","SIMOTICS SD motor type: 1CV2166B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing, increased power Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 160L, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 220 VD/380 VY IM B 3, without motor protection Terminal box at top",2455,"ΤΕΜ",1,"LVM",1,"1LE15011DB617AA4"]
["1LE1501-1DC23-4AA4","SIMOTICS SD motor type: 1CV2162C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 6-pole * frame size 160M, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box at top",1653,"ΤΕΜ",1,"LVM",1,"1LE15011DC234AA4"]
["1LE1501-1DD30-4JA4","SIMOTICS SD motor type: 1CV2163D low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, 8-pole * frame size 160M, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2220,"ΤΕΜ",1,"LVM",1,"1LE15011DD304JA4"]
["1LE1501-1EA23-4AA6","SIMOTICS SD motor type: 1CV2182A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 180M, * 22 kW (50 Hz) 24.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box on left-hand side",2904,"ΤΕΜ",1,"LVM",1,"1LE15011EA234AA6"]
["1LE1501-1EB22-7JA4","SIMOTICS SD motor type: 1CV2182B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 180M, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 500 VY 3 AC 60Hz 575VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2463,"ΤΕΜ",1,"LVM",1,"1LE15011EB227JA4"]
["1LE1501-1EB23-4AC4","SIMOTICS SD motor type: 1CV2182B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 180M, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",2518,"ΤΕΜ",1,"LVM",1,"1LE15011EB234AC4"]
["1LE1501-1EC42-1WB5","SIMOTICS SD motor type: 1CV2184C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 6-pole * frame size 180L, * 15 kW (50 Hz) 18 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 15 * Flange: FF300 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",3431,"ΤΕΜ",1,"LVM",1,"1LE15011EC421WB5"]
["1LE1501-1EC62-2JA4","SIMOTICS SD motor type: 1CV2186C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing, increased power Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 6-pole * frame size 180L, * 18.5 kW (50 Hz) 22 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",3714,"ΤΕΜ",1,"LVM",1,"1LE15011EC622JA4"]
["1LE1501-2AA41-8AA4","SIMOTICS SD motor type: 1CV2204A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 200L, * 30 kW (50 Hz) 33.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 230 VD/400 VY IM B 3, without motor protection Terminal box at top",3596,"ΤΕΜ",1,"LVM",1,"1LE15012AA418AA4"]
["1LE1501-2AA43-3JB5","SIMOTICS SD motor type: 1CV2204A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 200L, * 30 kW (50 Hz) 33.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",4167,"ΤΕΜ",1,"LVM",1,"1LE15012AA433JB5"]
["1LE1501-2AB50-2FA4","SIMOTICS SD motor type: 1CV2205B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 200L, * 30 kW (50 Hz) 34.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF350 (A400) without motor protection Terminal box at top",3631,"ΤΕΜ",1,"LVM",1,"1LE15012AB502FA4"]
["1LE1501-2AB53-4JA5","SIMOTICS SD motor type: 1CV2205B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 200L, * 30 kW (50 Hz) 34.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF350 (A400) without motor protection Terminal box on RHS",3908,"ΤΕΜ",1,"LVM",1,"1LE15012AB534JA5"]
["1LE1501-2AC43-1FA4","SIMOTICS SD motor type: 1CV2204C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, 60 Hz, P60: IE1 in EEA: minimum efficiency according to applicable statutory regulations to be considered 6-pole * frame size 200L, * 18.5 kW (50 Hz) 22 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60Hz 400VD/690VY IM B 5, flange: FF350 (A400) without motor protection Terminal box at top",3724,"ΤΕΜ",1,"LVM",1,"1LE15012AC431FA4"]
["1LE1501-2AC63-0FA4","SIMOTICS SD motor type: 1CV2206C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing, increased power Basic Line High Efficiency IE2, 6-pole * frame size 200L, * 30 kW (50 Hz) 34.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 380 VD/660 VY IM B 5, flange: FF350 (A400) without motor protection Terminal box at top",5767,"ΤΕΜ",1,"LVM",1,"1LE15012AC630FA4"]
["1LE1501-2BA22-1FB4","SIMOTICS SD motor type: 1CV2222A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 225M * 45 kW (50 Hz) 51 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF400 (A450) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",5588,"ΤΕΜ",1,"LVM",1,"1LE15012BA221FB4"]
["1LE1501-2BA63-3JA4","SIMOTICS SD motor type: 1CV2226A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing, increased power Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 225M * 55 kW (50 Hz) 62 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF400 (A450) without motor protection Terminal box at top",6484,"ΤΕΜ",1,"LVM",1,"1LE15012BA633JA4"]
["1LE1501-2BB01-8FA4","SIMOTICS SD motor type: 1CV2220B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 225S * 37 kW (50 Hz) 42.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 230 VD/400 VY IM B 5, flange: FF400 (A450) without motor protection Terminal box at top",4392,"ΤΕΜ",1,"LVM",1,"1LE15012BB018FA4"]
["1LE1501-2BB23-4WC4","SIMOTICS SD motor type: 1CV2222B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 225M * 45 kW (50 Hz) 52 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF400 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",5438,"ΤΕΜ",1,"LVM",1,"1LE15012BB234WC4"]
["1LE1501-2BC22-2AC6","SIMOTICS SD motor type: 1CV2222C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, 60 Hz, P60: IE1 in EEA: minimum efficiency according to applicable statutory regulations to be considered 6-pole * frame size 225M * 30 kW (50 Hz) 36 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",5767,"ΤΕΜ",1,"LVM",1,"1LE15012BC222AC6"]
["1LE1501-2BC23-4FB6","SIMOTICS SD motor type: 1CV2222C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, 60 Hz, P60: IE1 in EEA: minimum efficiency according to applicable statutory regulations to be considered 6-pole * frame size 225M * 30 kW (50 Hz) 36 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF400 (A450) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",5871,"ΤΕΜ",1,"LVM",1,"1LE15012BC234FB6"]
["1LE1501-2BD21-8FA4","SIMOTICS SD motor type: 1CV2222D low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, 8-pole * frame size 225M * 22 kW (50 Hz) 26.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 230 VD/400 VY IM B 5, flange: FF400 (A450) without motor protection Terminal box at top",5700,"ΤΕΜ",1,"LVM",1,"1LE15012BD218FA4"]
["1LE1501-2CA62-1FA4","SIMOTICS SD motor type: 1CV2256A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing, increased power Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 250M * 75 kW (50 Hz) 84 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF500 (A550) without motor protection Terminal box at top",8836,"ΤΕΜ",1,"LVM",1,"1LE15012CA621FA4"]
["1LE1501-2CB23-4AC4","SIMOTICS SD motor type: 1CV2252B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 250M * 55 kW (50 Hz) 63 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",6071,"ΤΕΜ",1,"LVM",1,"1LE15012CB234AC4"]
["1LE1501-2CC22-1AA5","SIMOTICS SD motor type: 1CV2252C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, 60 Hz, P60: IE1 in EEA: minimum efficiency according to applicable statutory regulations to be considered 6-pole * frame size 250M * 37 kW (50 Hz) 44.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B3 without motor protection Terminal box on RHS",6835,"ΤΕΜ",1,"LVM",1,"1LE15012CC221AA5"]
["1LE1501-2CD23-5JA4","SIMOTICS SD motor type: 1CV2252D low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, 8-pole * frame size 250M * 30 kW (50 Hz) 36 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 35 * Flange: FF500 (A550) without motor protection Terminal box at top",7495,"ΤΕΜ",1,"LVM",1,"1LE15012CD235JA4"]
["1LE1501-2DA04-0JA4","SIMOTICS SD motor type: 1CV2280A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 280S, * 75 kW (50 Hz) 84 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 500 VD 3 AC 60 Hz 575 VD IM B 35 * Flange: FF500 (A550) without motor protection Terminal box at top",8780,"ΤΕΜ",1,"LVM",1,"1LE15012DA040JA4"]
["1LE1501-2DA22-2AC6","SIMOTICS SD motor type: 1CV2282A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 280M * 90 kW (50 Hz) 101 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",10602,"ΤΕΜ",1,"LVM",1,"1LE15012DA222AC6"]
["1LE1501-2DA62-2FA4","SIMOTICS SD motor type: 1CV2286A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing, increased power Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 280M * 110 kW (50 Hz) 123 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF500 (A550) without motor protection Terminal box at top",12372,"ΤΕΜ",1,"LVM",1,"1LE15012DA622FA4"]
["1LE1501-2DB22-1GA4","SIMOTICS SD motor type: 1CV2282B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 280M * 90 kW (50 Hz) 104 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF500 (A550) without motor protection Terminal box at top",9673,"ΤΕΜ",1,"LVM",1,"1LE15012DB221GA4"]
["1LE1501-2DB63-0AA4","SIMOTICS SD motor type: 1CV2286B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing, increased power Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 280M * 110 kW (50 Hz) 127 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 380 VD/660 VY IM B 3, without motor protection Terminal box at top",11695,"ΤΕΜ",1,"LVM",1,"1LE15012DB630AA4"]
["1LE1501-2DC03-1JA4","SIMOTICS SD motor type: 1CV2280C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, 60 Hz, P60: IE1 in EEA: minimum efficiency according to applicable statutory regulations to be considered 6-pole * frame size 280S, * 45 kW (50 Hz) 54 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60Hz 400VD/690VY IM B 35 * Flange: FF500 (A550) without motor protection Terminal box at top",8279,"ΤΕΜ",1,"LVM",1,"1LE15012DC031JA4"]
["1LE1501-2DC23-4GB4","SIMOTICS SD motor type: 1CV2282C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, 60 Hz, P60: IE1 in EEA: minimum efficiency according to applicable statutory regulations to be considered 6-pole * frame size 280M * 55 kW (50 Hz) 66 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",9719,"ΤΕΜ",1,"LVM",1,"1LE15012DC234GB4"]
["1LE1501-2DD20-2JA4","SIMOTICS SD motor type: 1CV2282D low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, 8-pole * frame size 280M * 45 kW (50 Hz) 54 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF500 (A550) without motor protection Terminal box at top",10656,"ΤΕΜ",1,"LVM",1,"1LE15012DD202JA4"]
["1LE1501-3AA02-2FC6","SIMOTICS SD motor type: 1CV2310A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 315S, * 110 kW (50 Hz) 123 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, Flange: FF600 (A660) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",13093,"ΤΕΜ",1,"LVM",1,"1LE15013AA022FC6"]
["1LE1501-3AA42-1AA5","SIMOTICS SD motor type: 1CV2314A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 315L, * 160 kW (50 Hz) 180 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, without motor protection Terminal box on RHS",18244,"ΤΕΜ",1,"LVM",1,"1LE15013AA421AA5"]
["1LE1501-3AA53-4AA5","SIMOTICS SD motor type: 1CV2315A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 315L, * 200 kW (50 Hz) 224 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box on RHS",22302,"ΤΕΜ",1,"LVM",1,"1LE15013AA534AA5"]
["1LE1501-3AB03-3GA5","SIMOTICS SD motor type: 1CV2310B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 315S, * 110 kW (50 Hz) 127 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, Flange: FF600 (A660) without motor protection Terminal box on RHS",12698,"ΤΕΜ",1,"LVM",1,"1LE15013AB033GA5"]
["1LE1501-3AB22-1GA6","SIMOTICS SD motor type: 1CV2312B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 315M, * 132 kW (50 Hz) 152 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, Flange: FF600 (A660) without motor protection Terminal box on left-hand side",14835,"ΤΕΜ",1,"LVM",1,"1LE15013AB221GA6"]
["1LE1501-3AB43-3GA6","SIMOTICS SD motor type: 1CV2314B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 315L, * 160 kW (50 Hz) 184 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, Flange: FF600 (A660) without motor protection Terminal box on left-hand side",17597,"ΤΕΜ",1,"LVM",1,"1LE15013AB433GA6"]
["1LE1501-3AB53-1JA4","SIMOTICS SD motor type: 1CV2315B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 315L, * 200 kW (50 Hz) 230 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60Hz 400VD/690VY IM B 35 * Flange: FF600 (A660) without motor protection Terminal box at top",21128,"ΤΕΜ",1,"LVM",1,"1LE15013AB531JA4"]
["1LE1501-3AC02-2FA5","SIMOTICS SD motor type: 1CV2310C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, 60 Hz, P60: IE1 in EEA: minimum efficiency according to applicable statutory regulations to be considered 6-pole * frame size 315S, * 75 kW (50 Hz) 90 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, Flange: FF600 (A660) without motor protection Terminal box on RHS",13573,"ΤΕΜ",1,"LVM",1,"1LE15013AC022FA5"]
["1LE1501-3AC22-1JA4","SIMOTICS SD motor type: 1CV2312C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, 60 Hz, P60: IE1 in EEA: minimum efficiency according to applicable statutory regulations to be considered 6-pole * frame size 315M, * 90 kW (50 Hz) 108 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF600 (A660) without motor protection Terminal box at top",14912,"ΤΕΜ",1,"LVM",1,"1LE15013AC221JA4"]
["1LE1501-3AC50-2AA4","SIMOTICS SD motor type: 1CV2315C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 6-pole * frame size 315L, * 132 kW (50 Hz) 158 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B 3, without motor protection Terminal box at top",20169,"ΤΕΜ",1,"LVM",1,"1LE15013AC502AA4"]
["1LE1501-3AC62-2GB6","SIMOTICS SD motor type: 1CV2316C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 6-pole * frame size 315L, * 160 kW (50 Hz) 192 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",25672,"ΤΕΜ",1,"LVM",1,"1LE15013AC622GB6"]
["1LE1501-3AD22-1FA4","SIMOTICS SD motor type: 1CV2312D low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, 8-pole * frame size 315M, * 75 kW (50 Hz) 90 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, Flange: FF600 (A660) without motor protection Terminal box at top",16866,"ΤΕΜ",1,"LVM",1,"1LE15013AD221FA4"]
["1LE1503-0CA23-5AA4","SIMOTICS SD motor type: 1CV3072A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 71M * 0.37 kW (50 Hz) 0.43 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 3, without motor protection Terminal box at top",365,"ΤΕΜ",1,"LVM",1,"1LE15030CA235AA4"]
["1LE1503-0CB22-2JA4","SIMOTICS SD motor type: 1CV3072B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 4-pole * frame size 71M * 0.25 kW (50 Hz) 0.29 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF130 (A160) without motor protection Terminal box at top",372,"ΤΕΜ",1,"LVM",1,"1LE15030CB222JA4"]
["1LE1503-0CB32-3JA4","SIMOTICS SD motor type: 1CV3073B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 4-pole * frame size 71M * 0.37 kW (50 Hz) 0.43 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 240 VD/415 VY 3 AC 60 Hz 480 VY IM B 35 * Flange: FF130 (A160) without motor protection Terminal box at top",431,"ΤΕΜ",1,"LVM",1,"1LE15030CB323JA4"]
["1LE1503-0DA22-2GB6","SIMOTICS SD motor type: 1CV3082A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 80M * 0.75 kW (50 Hz) 0.86 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF165 (A200) 1 PTC thermistor for disconnection (2 terminals) Terminal box on left-hand side",497,"ΤΕΜ",1,"LVM",1,"1LE15030DA222GB6"]
["1LE1503-0DB20-4FA4","SIMOTICS SD motor type: 1CV3082B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 4-pole * frame size 80M * 0.55 kW (50 Hz) 0.63 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF165 (A200) without motor protection Terminal box at top",445,"ΤΕΜ",1,"LVM",1,"1LE15030DB204FA4"]
["1LE1503-0DB32-2AA4","SIMOTICS SD motor type: 1CV3083B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 4-pole * frame size 80M * 0.75 kW (50 Hz) 0.86 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, without motor protection Terminal box at top",454,"ΤΕΜ",1,"LVM",1,"1LE15030DB322AA4"]
["1LE1503-0DC33-5JA4","SIMOTICS SD motor type: 1CV3083C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 80M * 0.55 kW (50 Hz) 0.63 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 35 * Flange: FF165 (A200) without motor protection Terminal box at top",514,"ΤΕΜ",1,"LVM",1,"1LE15030DC335JA4"]
["1LE1503-0EB03-0JA4","SIMOTICS SD motor type: 1CV3090B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 4-pole * frame size 90S * 1.1 kW (50 Hz) 1.27 kW (60 Hz) 60 Hz, P60: IE2 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 380 VD/660 VY IM B 35 * Flange: FF165 (A200) without motor protection Terminal box at top",595,"ΤΕΜ",1,"LVM",1,"1LE15030EB030JA4"]
["1LE1503-1AA42-1JB5","SIMOTICS SD motor type: 1CV3104A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * frame size 100L * 3 kW (50 Hz) 3.45 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",862,"ΤΕΜ",1,"LVM",1,"1LE15031AA421JB5"]
["1LE1503-1AB53-0AA4","SIMOTICS SD motor type: 1CV3105B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 4-pole * frame size 100L * 3 kW (50 Hz) 3.45 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 380 VD/660 VY IM B 3, without motor protection Terminal box at top",731,"ΤΕΜ",1,"LVM",1,"1LE15031AB530AA4"]
["1LE1503-1BA22-1JB7","SIMOTICS SD motor type: 1CV3112A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * frame size 112M, * 4 kW (50 Hz) 4.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",1002,"ΤΕΜ",1,"LVM",1,"1LE15031BA221JB7"]
["1LE1503-1CA12-2AC4","SIMOTICS SD motor type: 1CV3131A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 132S, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",1408,"ΤΕΜ",1,"LVM",1,"1LE15031CA122AC4"]
["1LE1503-1CB23-5FA4","SIMOTICS SD motor type: 1CV3132B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 132M, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 5, flange: FF265 (A300) without motor protection Terminal box at top",1471,"ΤΕΜ",1,"LVM",1,"1LE15031CB235FA4"]
["1LE1503-1DA23-3AA4","SIMOTICS SD motor type: 1CV3162A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 160M, * 11 kW (50 Hz) 12.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, without motor protection Terminal box at top",1789,"ΤΕΜ",1,"LVM",1,"1LE15031DA233AA4"]
["1LE1503-1DA23-4GA5","SIMOTICS SD motor type: 1CV3162A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 160M, * 11 kW (50 Hz) 12.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) without motor protection Terminal box on RHS",1893,"ΤΕΜ",1,"LVM",1,"1LE15031DA234GA5"]
["1LE1503-1DA40-4GB6","SIMOTICS SD motor type: 1CV3164A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 160L, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",2952,"ΤΕΜ",1,"LVM",1,"1LE15031DA404GB6"]
["1LE1503-1DA43-4AA6","SIMOTICS SD motor type: 1CV3164A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 160L, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box on left-hand side",2770,"ΤΕΜ",1,"LVM",1,"1LE15031DA434AA6"]
["1LE1503-1DB62-7FA4","SIMOTICS SD motor type: 1CV3166B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing, increased power Basic Line Premium Efficiency IE3, 4-pole * frame size 160L, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 500 VY 3 AC 60Hz 575VY IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",2778,"ΤΕΜ",1,"LVM",1,"1LE15031DB627FA4"]
["1LE1503-1EA23-4GC4","SIMOTICS SD motor type: 1CV3182A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 180M, * 22 kW (50 Hz) 24.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",3346,"ΤΕΜ",1,"LVM",1,"1LE15031EA234GC4"]
["1LE1503-1EB22-2AC5","SIMOTICS SD motor type: 1CV3182B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 4-pole * frame size 180M, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) 60 Hz, P60: IE2 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",2951,"ΤΕΜ",1,"LVM",1,"1LE15031EB222AC5"]
["1LE1503-1EB23-3WB6","SIMOTICS SD motor type: 1CV3182B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 4-pole * frame size 180M, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) 60 Hz, P60: IE2 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 15 * Flange: FF300 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",3087,"ΤΕΜ",1,"LVM",1,"1LE15031EB233WB6"]
["1LE1503-1EC40-4GB5","SIMOTICS SD motor type: 1CV3184C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 180L, * 15 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",3606,"ΤΕΜ",1,"LVM",1,"1LE15031EC404GB5"]
["1LE1503-1EC43-3JA6","SIMOTICS SD motor type: 1CV3184C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 180L, * 15 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF300 (A350) without motor protection Terminal box on left-hand side",3578,"ΤΕΜ",1,"LVM",1,"1LE15031EC433JA6"]
["1LE1503-2AA42-2AC5","SIMOTICS SD motor type: 1CV3204A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 200L, * 30 kW (50 Hz) 33.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",4325,"ΤΕΜ",1,"LVM",1,"1LE15032AA422AC5"]
["1LE1503-2AA43-3GA6","SIMOTICS SD motor type: 1CV3204A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 200L, * 30 kW (50 Hz) 33.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF350 (A400) without motor protection Terminal box on left-hand side",4357,"ΤΕΜ",1,"LVM",1,"1LE15032AA433GA6"]
["1LE1503-2AB50-4GB4","SIMOTICS SD motor type: 1CV3205B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 200L, * 30 kW (50 Hz) 34.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",4119,"ΤΕΜ",1,"LVM",1,"1LE15032AB504GB4"]
["1LE1503-2AB52-2GC4","SIMOTICS SD motor type: 1CV3205B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 200L, * 30 kW (50 Hz) 34.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF350 (A400) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",4214,"ΤΕΜ",1,"LVM",1,"1LE15032AB522GC4"]
["1LE1503-2AC40-4GA6","SIMOTICS SD motor type: 1CV3204C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 200L, * 18.5 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF350 (A400) without motor protection Terminal box on left-hand side",4243,"ΤΕΜ",1,"LVM",1,"1LE15032AC404GA6"]
["1LE1503-2AC52-1JB6","SIMOTICS SD motor type: 1CV3205C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 200L, * 22 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",5105,"ΤΕΜ",1,"LVM",1,"1LE15032AC521JB6"]
["1LE1503-2AC53-4WB5","SIMOTICS SD motor type: 1CV3205C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 200L, * 22 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF350 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",5053,"ΤΕΜ",1,"LVM",1,"1LE15032AC534WB5"]
["1LE1503-2BA23-4AA5","SIMOTICS SD motor type: 1CV3222A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 225M * 45 kW (50 Hz) 51 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box on RHS",5742,"ΤΕΜ",1,"LVM",1,"1LE15032BA234AA5"]
["1LE1503-2BA23-4JB4","SIMOTICS SD motor type: 1CV3222A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 225M * 45 kW (50 Hz) 51 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF400 (A450) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",5916,"ΤΕΜ",1,"LVM",1,"1LE15032BA234JB4"]
["1LE1503-2BB22-1GB6","SIMOTICS SD motor type: 1CV3222B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 225M * 45 kW (50 Hz) 52 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF400 (A450) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",5927,"ΤΕΜ",1,"LVM",1,"1LE15032BB221GB6"]
["1LE1503-2BB23-3JB6","SIMOTICS SD motor type: 1CV3222B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 225M * 45 kW (50 Hz) 52 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF400 (A450) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",5979,"ΤΕΜ",1,"LVM",1,"1LE15032BB233JB6"]
["1LE1503-2BC21-7FA4","SIMOTICS SD motor type: 1CV3222C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 225M * 30 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 220 VD/380 VY IM B 5, flange: FF400 (A450) without motor protection Terminal box at top",5961,"ΤΕΜ",1,"LVM",1,"1LE15032BC217FA4"]
["1LE1503-2BC23-4FA6","SIMOTICS SD motor type: 1CV3222C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 225M * 30 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF400 (A450) without motor protection Terminal box on left-hand side",6118,"ΤΕΜ",1,"LVM",1,"1LE15032BC234FA6"]
["1LE1503-2CA23-4FC4","SIMOTICS SD motor type: 1CV3252A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 250M * 55 kW (50 Hz) 62 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF500 (A550) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",7117,"ΤΕΜ",1,"LVM",1,"1LE15032CA234FC4"]
["1LE1503-2CB22-1FA6","SIMOTICS SD motor type: 1CV3252B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 250M * 55 kW (50 Hz) 63 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF500 (A550) without motor protection Terminal box on left-hand side",6995,"ΤΕΜ",1,"LVM",1,"1LE15032CB221FA6"]
["1LE1503-2CB23-4JB6","SIMOTICS SD motor type: 1CV3252B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 250M * 55 kW (50 Hz) 63 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",7155,"ΤΕΜ",1,"LVM",1,"1LE15032CB234JB6"]
["1LE1503-2CC23-5FA4","SIMOTICS SD motor type: 1CV3252C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 250M * 37 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 5, flange: FF500 (A550) without motor protection Terminal box at top",7324,"ΤΕΜ",1,"LVM",1,"1LE15032CC235FA4"]
["1LE1503-2DA03-3JB6","SIMOTICS SD motor type: 1CV3280A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * frame size 280S, * 75 kW (50 Hz) 84 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",10128,"ΤΕΜ",1,"LVM",1,"1LE15032DA033JB6"]
["1LE1503-2DA03-4JA4","SIMOTICS SD motor type: 1CV3280A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * frame size 280S, * 75 kW (50 Hz) 84 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF500 (A550) without motor protection Terminal box at top",9301,"ΤΕΜ",1,"LVM",1,"1LE15032DA034JA4"]
["1LE1503-2DB02-1FB4","SIMOTICS SD motor type: 1CV3280B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 280S, * 75 kW (50 Hz) 86 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",9100,"ΤΕΜ",1,"LVM",1,"1LE15032DB021FB4"]
["1LE1503-2DB03-3FB6","SIMOTICS SD motor type: 1CV3280B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 280S, * 75 kW (50 Hz) 86 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 5, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",9550,"ΤΕΜ",1,"LVM",1,"1LE15032DB033FB6"]
["1LE1503-2DB22-1JA6","SIMOTICS SD motor type: 1CV3282B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 280M * 90 kW (50 Hz) 104 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF500 (A550) without motor protection Terminal box on left-hand side",10906,"ΤΕΜ",1,"LVM",1,"1LE15032DB221JA6"]
["1LE1503-2DB61-8AA4","SIMOTICS SD motor type: 1CV3286B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing, increased power Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 280M * 110 kW (50 Hz) 127 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 230 VD/400 VY IM B 3, without motor protection Terminal box at top",13025,"ΤΕΜ",1,"LVM",1,"1LE15032DB618AA4"]
["1LE1503-2DC02-2WC4","SIMOTICS SD motor type: 1CV3280C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 280S, * 45 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 15 * Flange: FF500 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",9344,"ΤΕΜ",1,"LVM",1,"1LE15032DC022WC4"]
["1LE1503-2DC22-2JA6","SIMOTICS SD motor type: 1CV3282C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 280M * 55 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF500 (A550) without motor protection Terminal box on left-hand side",10741,"ΤΕΜ",1,"LVM",1,"1LE15032DC222JA6"]
["1LE1503-3AA02-1AA4","SIMOTICS SD motor type: 1CV3310A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 315S, * 110 kW (50 Hz) 123 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, without motor protection Terminal box at top",12723,"ΤΕΜ",1,"LVM",1,"1LE15033AA021AA4"]
["1LE1503-3AA22-2JA6","SIMOTICS SD motor type: 1CV3312A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 315M, * 132 kW (50 Hz) 148 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF600 (A660) without motor protection Terminal box on left-hand side",16153,"ΤΕΜ",1,"LVM",1,"1LE15033AA222JA6"]
["1LE1503-3AA42-2JC6","SIMOTICS SD motor type: 1CV3314A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * frame size 315L, * 160 kW (50 Hz) 180 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF600 (A660) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",20103,"ΤΕΜ",1,"LVM",1,"1LE15033AA422JC6"]
["1LE1503-3AA52-1GA5","SIMOTICS SD motor type: 1CV3315A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 315L, * 200 kW (50 Hz) 224 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, Flange: FF600 (A660) without motor protection Terminal box on RHS",24758,"ΤΕΜ",1,"LVM",1,"1LE15033AA521GA5"]
["1LE1503-3AA53-4AB6","SIMOTICS SD motor type: 1CV3315A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 315L, * 200 kW (50 Hz) 224 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",23973,"ΤΕΜ",1,"LVM",1,"1LE15033AA534AB6"]
["1LE1503-3AB22-1AA5","SIMOTICS SD motor type: 1CV3312B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 4-pole * frame size 315M, * 132 kW (50 Hz) 152 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, without motor protection Terminal box on RHS",15169,"ΤΕΜ",1,"LVM",1,"1LE15033AB221AA5"]
["1LE1503-3AB23-4FC4","SIMOTICS SD motor type: 1CV3312B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 4-pole * frame size 315M, * 132 kW (50 Hz) 152 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, Flange: FF600 (A660) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",15338,"ΤΕΜ",1,"LVM",1,"1LE15033AB234FC4"]
["1LE1503-3AB43-3GA6","SIMOTICS SD motor type: 1CV3314B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 4-pole * frame size 315L, * 160 kW (50 Hz) 184 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, Flange: FF600 (A660) without motor protection Terminal box on left-hand side",18796,"ΤΕΜ",1,"LVM",1,"1LE15033AB433GA6"]
["1LE1503-3AB53-3AB6","SIMOTICS SD motor type: 1CV3315B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 315L, * 200 kW (50 Hz) 230 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",22677,"ΤΕΜ",1,"LVM",1,"1LE15033AB533AB6"]
["1LE1503-3AC03-4FA5","SIMOTICS SD motor type: 1CV3310C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 315S, * 75 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, Flange: FF600 (A660) without motor protection Terminal box on RHS",14355,"ΤΕΜ",1,"LVM",1,"1LE15033AC034FA5"]
["1LE1503-3AC52-2JC4","SIMOTICS SD motor type: 1CV3315C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 315L, * 132 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF600 (A660) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",22451,"ΤΕΜ",1,"LVM",1,"1LE15033AC522JC4"]
["1LE1504-1AA42-1JA4","SIMOTICS SD motor type: 1CV4104A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 2-pole * frame size 100L * 3 kW (50 Hz) 3.45 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF215 (A250) without motor protection Terminal box at top",880,"ΤΕΜ",1,"LVM",1,"1LE15041AA421JA4"]
["1LE1504-1CA02-1JA4","SIMOTICS SD motor type: 1CV4130A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 2-pole * frame size 132S, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF265 (A300) without motor protection Terminal box at top",1308,"ΤΕΜ",1,"LVM",1,"1LE15041CA021JA4"]
["1LE1504-1DA40-4GB6","SIMOTICS SD motor type: 1CV4164A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 2-pole * frame size 160L, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",3520,"ΤΕΜ",1,"LVM",1,"1LE15041DA404GB6"]
["1LE1504-1DA43-3GA4","SIMOTICS SD motor type: 1CV4164A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 2-pole * frame size 160L, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF300 (A350) without motor protection Terminal box at top",3411,"ΤΕΜ",1,"LVM",1,"1LE15041DA433GA4"]
["1LE1504-1EA23-3FB5","SIMOTICS SD motor type: 1CV4182A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 2-pole * frame size 180M, * 22 kW (50 Hz) 24.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",4158,"ΤΕΜ",1,"LVM",1,"1LE15041EA233FB5"]
["1LE1504-1EB22-2WC4","SIMOTICS SD motor type: 1CV4182B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 4-pole * frame size 180M, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 15 * Flange: FF300 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",3484,"ΤΕΜ",1,"LVM",1,"1LE15041EB222WC4"]
["1LE1504-1EB23-4JA4","SIMOTICS SD motor type: 1CV4182B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 4-pole * frame size 180M, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",3239,"ΤΕΜ",1,"LVM",1,"1LE15041EB234JA4"]
["1LE1504-1EB42-2JB5","SIMOTICS SD motor type: 1CV4184B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 4-pole * frame size 180L, * 22 kW (50 Hz) 25.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",4026,"ΤΕΜ",1,"LVM",1,"1LE15041EB422JB5"]
["1LE1504-2AA40-4JB5","SIMOTICS SD motor type: 1CV4204A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 2-pole * frame size 200L, * 30 kW (50 Hz) 33.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",5189,"ΤΕΜ",1,"LVM",1,"1LE15042AA404JB5"]
["1LE1504-2AA50-4GB5","SIMOTICS SD motor type: 1CV4205A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 2-pole * frame size 200L, * 37 kW (50 Hz) 41.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",6306,"ΤΕΜ",1,"LVM",1,"1LE15042AA504GB5"]
["1LE1504-2AA53-4AA6","SIMOTICS SD motor type: 1CV4205A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 2-pole * frame size 200L, * 37 kW (50 Hz) 41.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box on left-hand side",6013,"ΤΕΜ",1,"LVM",1,"1LE15042AA534AA6"]
["1LE1504-2AB52-1GB4","SIMOTICS SD motor type: 1CV4205B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 4-pole * frame size 200L, * 30 kW (50 Hz) 34.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",4942,"ΤΕΜ",1,"LVM",1,"1LE15042AB521GB4"]
["1LE1504-2BA22-2JA6","SIMOTICS SD motor type: 1CV4222A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 2-pole * frame size 225M * 45 kW (50 Hz) 51 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF400 (A450) without motor protection Terminal box on left-hand side",6850,"ΤΕΜ",1,"LVM",1,"1LE15042BA222JA6"]
["1LE1504-2BB00-4JA4","SIMOTICS SD motor type: 1CV4220B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 4-pole * frame size 225S * 37 kW (50 Hz) 42.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF400 (A450) without motor protection Terminal box at top",5371,"ΤΕΜ",1,"LVM",1,"1LE15042BB004JA4"]
["1LE1504-2BB03-4JB5","SIMOTICS SD motor type: 1CV4220B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 4-pole * frame size 225S * 37 kW (50 Hz) 42.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF400 (A450) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",5810,"ΤΕΜ",1,"LVM",1,"1LE15042BB034JB5"]
["1LE1504-2BB23-4GB5","SIMOTICS SD motor type: 1CV4222B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 60 Hz, P60: IE3 4-pole * frame size 225M * 45 kW (50 Hz) 52 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF400 (A450) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",6601,"ΤΕΜ",1,"LVM",1,"1LE15042BB234GB5"]
["1LE1504-2CA22-1GB4","SIMOTICS SD motor type: 1CV4252A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 2-pole * frame size 250M * 55 kW (50 Hz) 62 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",8072,"ΤΕΜ",1,"LVM",1,"1LE15042CA221GB4"]
["1LE1504-2CA23-4FC4","SIMOTICS SD motor type: 1CV4252A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 2-pole * frame size 250M * 55 kW (50 Hz) 62 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF500 (A550) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",8055,"ΤΕΜ",1,"LVM",1,"1LE15042CA234FC4"]
["1LE1504-2CB22-2GB4","SIMOTICS SD motor type: 1CV4252B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 4-pole * frame size 250M * 55 kW (50 Hz) 63 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",7631,"ΤΕΜ",1,"LVM",1,"1LE15042CB222GB4"]
["1LE1504-2DA02-2WB5","SIMOTICS SD motor type: 1CV4280A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 2-pole * frame size 280S, * 75 kW (50 Hz) 84 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 15 * Flange: FF500 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",11528,"ΤΕΜ",1,"LVM",1,"1LE15042DA022WB5"]
["1LE1504-2DA22-1AB5","SIMOTICS SD motor type: 1CV4282A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 2-pole * frame size 280M * 90 kW (50 Hz) 101 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",12814,"ΤΕΜ",1,"LVM",1,"1LE15042DA221AB5"]
["1LE1504-2DB02-1JB4","SIMOTICS SD motor type: 1CV4280B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 4-pole * frame size 280S, * 75 kW (50 Hz) 86 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",10512,"ΤΕΜ",1,"LVM",1,"1LE15042DB021JB4"]
["1LE1504-2DB20-4JB6","SIMOTICS SD motor type: 1CV4282B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 4-pole * frame size 280M * 90 kW (50 Hz) 104 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",12308,"ΤΕΜ",1,"LVM",1,"1LE15042DB204JB6"]
["1LE1504-3AA00-4GA6","SIMOTICS SD motor type: 1CV4310A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 2-pole * frame size 315S, * 110 kW (50 Hz) 123 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, Flange: FF600 (A660) without motor protection Terminal box on left-hand side",15246,"ΤΕΜ",1,"LVM",1,"1LE15043AA004GA6"]
["1LE1504-3AA22-3JA4","SIMOTICS SD motor type: 1CV4312A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 2-pole * frame size 315M, * 132 kW (50 Hz) 148 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 240VD/415VY * 3 AC 60 Hz 480 VY IM B 35 * Flange: FF600 (A660) without motor protection Terminal box at top",17778,"ΤΕΜ",1,"LVM",1,"1LE15043AA223JA4"]
["1LE1504-3AA23-4GC4","SIMOTICS SD motor type: 1CV4312A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 2-pole * frame size 315M, * 132 kW (50 Hz) 148 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, Flange: FF600 (A660) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",17844,"ΤΕΜ",1,"LVM",1,"1LE15043AA234GC4"]
["1LE1504-3AB20-4AB6","SIMOTICS SD motor type: 1CV4312B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 4-pole * frame size 315M, * 132 kW (50 Hz) 152 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",16990,"ΤΕΜ",1,"LVM",1,"1LE15043AB204AB6"]
["1LE1504-3AB23-4GB4","SIMOTICS SD motor type: 1CV4312B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 4-pole * frame size 315M, * 132 kW (50 Hz) 152 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",17025,"ΤΕΜ",1,"LVM",1,"1LE15043AB234GB4"]
["1LE1504-3AB52-2JB5","SIMOTICS SD motor type: 1CV4315B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 4-pole * frame size 315L, * 200 kW (50 Hz) 230 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",25849,"ΤΕΜ",1,"LVM",1,"1LE15043AB522JB5"]
["1LE1601-1EB22-2AC4","SIMOTICS SD motor type: 1CV2182B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 180M, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",2748,"ΤΕΜ",1,"LVM",1,"1LE16011EB222AC4"]
["1LE1601-2AB53-4GB5","SIMOTICS SD motor type: 1CV2205B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 200L, * 30 kW (50 Hz) 34.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",4207,"ΤΕΜ",1,"LVM",1,"1LE16012AB534GB5"]
["1LE1601-2BC20-4JB6","SIMOTICS SD motor type: 1CV2222C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line High Efficiency IE2, 60 Hz, P60: IE1 in EEA: minimum efficiency according to applicable statutory regulations to be considered 6-pole * frame size 225M * 30 kW (50 Hz) 36 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF400 (A450) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",6276,"ΤΕΜ",1,"LVM",1,"1LE16012BC204JB6"]
["1LE1601-2BC22-2GC5","SIMOTICS SD motor type: 1CV2222C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line High Efficiency IE2, 60 Hz, P60: IE1 in EEA: minimum efficiency according to applicable statutory regulations to be considered 6-pole * frame size 225M * 30 kW (50 Hz) 36 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF400 (A450) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",6509,"ΤΕΜ",1,"LVM",1,"1LE16012BC222GC5"]
["1LE1601-2DB23-3AB4","SIMOTICS SD motor type: 1CV2282B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 280M * 90 kW (50 Hz) 104 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",9651,"ΤΕΜ",1,"LVM",1,"1LE16012DB233AB4"]
["1LE1601-3AA03-3GB4","SIMOTICS SD motor type: 1CV2310A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 315S, * 110 kW (50 Hz) 123 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",13171,"ΤΕΜ",1,"LVM",1,"1LE16013AA033GB4"]
["1LE1601-3AA52-2AC5","SIMOTICS SD motor type: 1CV2315A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 315L, * 200 kW (50 Hz) 224 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",23803,"ΤΕΜ",1,"LVM",1,"1LE16013AA522AC5"]
["1LE1601-3AB43-4AC4","SIMOTICS SD motor type: 1CV2314B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 315L, * 160 kW (50 Hz) 184 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",17188,"ΤΕΜ",1,"LVM",1,"1LE16013AB434AC4"]
["1LE1603-1AA42-2GB4","SIMOTICS SD motor type: 1CV3104A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * frame size 100L * 3 kW (50 Hz) 3.45 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",786,"ΤΕΜ",1,"LVM",1,"1LE16031AA422GB4"]
["1LE1603-1CA02-2JC5","SIMOTICS SD motor type: 1CV3130A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line Premium Efficiency IE3, 2-pole * frame size 132S, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) 60 Hz, P60: IE2 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",1393,"ΤΕΜ",1,"LVM",1,"1LE16031CA022JC5"]
["1LE1603-1DA32-2GC7","SIMOTICS SD motor type: 1CV3163A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line Premium Efficiency IE3, 2-pole * frame size 160M, * 15 kW (50 Hz) 17.3 kW (60 Hz) 60 Hz, P60: IE2 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",2856,"ΤΕΜ",1,"LVM",1,"1LE16031DA322GC7"]
["1LE1603-2AB52-2GB4","SIMOTICS SD motor type: 1CV3205B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 200L, * 30 kW (50 Hz) 34.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",4328,"ΤΕΜ",1,"LVM",1,"1LE16032AB522GB4"]
["1LE1603-2BC22-2GC5","SIMOTICS SD motor type: 1CV3222C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line Premium Efficiency IE3, 6-pole * frame size 225M * 30 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF400 (A450) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",6874,"ΤΕΜ",1,"LVM",1,"1LE16032BC222GC5"]
["1LE1603-2CC22-2AC5","SIMOTICS SD motor type: 1CV3252C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line Premium Efficiency IE3, 6-pole * frame size 250M * 37 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",8139,"ΤΕΜ",1,"LVM",1,"1LE16032CC222AC5"]
["1LE1603-3AB22-1JB5","SIMOTICS SD motor type: 1CV3312B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line Premium Efficiency IE3, 4-pole * frame size 315M, * 132 kW (50 Hz) 152 kW (60 Hz) 60 Hz, P60: IE2 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",16263,"ΤΕΜ",1,"LVM",1,"1LE16033AB221JB5"]
["1LE1603-3AC03-3JB6","SIMOTICS SD motor type: 1CV3310C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line Premium Efficiency IE3, 6-pole * frame size 315S, * 75 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",15065,"ΤΕΜ",1,"LVM",1,"1LE16033AC033JB6"]
["1LE5503-3AA63-4GC5","SIMOTICS SD motor type: 1CV3316A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 315L* 250 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1, Flange: FF740 (A800) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",28961,"ΤΕΜ",1,"LVM",1,"1LE55033AA634GC5"]
["1LE5504-3AA63-4JA0","SIMOTICS SD motor type: 1CV4316A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE4 2-pole * frame size 315L* 250 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF740 (A800) without motor protection Terminal box base left with terminal box at top",32119,"ΤΕΜ",1,"LVM",1,"1LE55043AA634JA0"]
["1LE5604-3AA63-3FB0","SIMOTICS SD motor type: 1CV4316A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Performance Line Premium Efficiency IE4 2-pole * frame size 315L* 250 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 5, Flange: FF740 (A800) 3 PTC thermistors for disconnection (2 terminals) Terminal box base left with terminal box at top",33246,"ΤΕΜ",1,"LVM",1,"1LE56043AA633FB0"]
["1LE5604-3BA33-4FB5","SIMOTICS SD motor type: 1CV4353A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Performance Line Premium Efficiency IE4 2-pole * frame size 355L * 355 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, Flange: FF840 (A900) disconnection (2 terminals) Terminal box on RHS",48275,"ΤΕΜ",1,"LVM",1,"1LE56043BA334FB5"]
["1MB1011-1CC33-4HA4","SIMOTICS XP motor type: 1AV2133C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP65 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2 6-pole * frame size 132M * 5.5 kW (50 Hz) 6.3 kW (60 Hz) version for zone 21 and zone 22 with conductive dust standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V3, flange: FF265 (A300) without motor protection Terminal box at top",1522,"ΤΕΜ",1,"LVM",1,"1MB10111CC334HA4"]
["1MB1021-1BC23-4AA4","SIMOTICS XP motor type: 1AV2112C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2 6-pole * frame size 112M * 2.2 kW (50 Hz) 2.55 kW (60 Hz) version for zone 22 for non-conductive dust standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 without motor protection Terminal box at top",723,"ΤΕΜ",1,"LVM",1,"1MB10211BC234AA4"]
["1MB1021-1CC23-4HA4","SIMOTICS XP motor type: 1AV2132C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2 6-pole * frame size 132M * 4 kW (50 Hz) 4.55 kW (60 Hz) version for zone 22 for non-conductive dust standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V3, flange: FF265 (A300) without motor protection Terminal box at top",1185,"ΤΕΜ",1,"LVM",1,"1MB10211CC234HA4"]
["1MB1031-1BC22-2FA4","SIMOTICS XP motor type: 1AV2112C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2 6-pole * frame size 112M * 2.2 kW (50 Hz) 2.55 kW (60 Hz) Ex ec IIC T3 Gc version for zone 2 according to IEC/EN 60 079-7 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B5, flange: FF215 (A250) without motor protection Terminal box at top",815,"ΤΕΜ",1,"LVM",1,"1MB10311BC222FA4"]
["1MB1031-1DC42-2HB4","SIMOTICS XP motor type: 1AV2164C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2 6-pole * frame size 160L * 11 kW (50 Hz) 12.6 kW (60 Hz) Ex ec IIC T3 Gc version for zone 2 according to IEC/EN 60 079-7 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V3, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2605,"ΤΕΜ",1,"LVM",1,"1MB10311DC422HB4"]
["1MB1513-0DC22-2FB4","SIMOTICS XP motor type: 1CV3082C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP65 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 80M * 0.37 kW (50 Hz), 0.43 kW (60 Hz) Ex tb IIIC T120Β° Db version for zone 21 and zone 22 with conductive dust standard color RAL 7030, if no order code is specified for selecting another color. 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM B 5, flange: FF165 (A200) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",564,"ΤΕΜ",1,"LVM",1,"1MB15130DC222FB4"]
["1MB1513-1CA12-2FA4","SIMOTICS XP motor type: 1CV3131A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP65 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 132S * 7.5 kW (50 Hz), 8.6 kW (60 Hz) Ex tb IIIC T120Β° Db version for zone 21 and zone 22 with conductive dust standard color RAL 7030, if no order code is specified for selecting another color. 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM B5, flange: FF265 (A300) without motor protection Terminal box at top",1571,"ΤΕΜ",1,"LVM",1,"1MB15131CA122FA4"]
["1MB1521-1CC22-2FB4","SIMOTICS XP motor type: 1CV2132C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2 6-pole * frame size 132M * 4 kW (50 Hz), 4.55 kW (60 Hz) Ex tc IIIB T120Β° Dc version for zone 22 for non-conductive dust standard color RAL 7030, if no order code is specified for selecting another color. 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM B5, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1367,"ΤΕΜ",1,"LVM",1,"1MB15211CC222FB4"]
["1MB1523-1BC23-4HB4","SIMOTICS XP motor type: 1CV3112C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 112M * 2.2 kW (50 Hz), 2.55 kW (60 Hz) P60:IE2 Ex tc IIIB T120Β° Dc version for zone 22 for non-conductive dust standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V3, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",987,"ΤΕΜ",1,"LVM",1,"1MB15231BC234HB4"]
["1MB1533-0EA42-2FB4","SIMOTICS XP motor type: 1CV3094A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 90L * 2.2 kW (50 Hz), 2.55 kW (60 Hz) Ex ec IIC T3 Gc version for zone 2 according to IEC/EN 60 079-7 standard color RAL 7030, if no order code is specified for selecting another color. 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM B 5, flange: FF165 (A200) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",820,"ΤΕΜ",1,"LVM",1,"1MB15330EA422FB4"]
["1LE1001-1AA42-1JB4","SIMOTICS GP motor type: 1AV2104A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * frame size 100L * 3 kW (50 Hz) 3.45 kW (60 Hz) 3 kW (60 Hz), 50 Hz power standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",678,"ΤΕΜ",1,"LVM",1,"1LE10011AA421JB4"]
["1LE1001-1AB42-1GB4","SIMOTICS GP motor type: 1AV2104B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * frame size 100L * 2.2 kW (50 Hz) 2.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",627,"ΤΕΜ",1,"LVM",1,"1LE10011AB421GB4"]
["1LE1001-1AB52-1GA5","SIMOTICS GP motor type: 1AV2105B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * frame size 100L * 3 kW (50 Hz) 3.45 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF215 (A250) without motor protection Terminal box on RHS",692,"ΤΕΜ",1,"LVM",1,"1LE10011AB521GA5"]
["1LE1001-1BA20-4GB5","SIMOTICS GP motor type: 1AV2112A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * frame size 112M, * 4 kW (50 Hz) 4.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",818,"ΤΕΜ",1,"LVM",1,"1LE10011BA204GB5"]
["1LE1001-1BB22-1GA4","SIMOTICS GP motor type: 1AV2112B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * frame size 112M, * 4 kW (50 Hz) 4.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF215 (A250) without motor protection Terminal box at top",789,"ΤΕΜ",1,"LVM",1,"1LE10011BB221GA4"]
["1LE1001-1BB23-4GA7","SIMOTICS GP motor type: 1AV2112B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * frame size 112M, * 4 kW (50 Hz) 4.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF215 (A250) without motor protection Terminal box below",813,"ΤΕΜ",1,"LVM",1,"1LE10011BB234GA7"]
["1LE1001-1CA03-4FC4","SIMOTICS GP motor type: 1AV2130A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 2-pole * frame size 132S, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",1016,"ΤΕΜ",1,"LVM",1,"1LE10011CA034FC4"]
["1LE1001-1CA13-4AC4","SIMOTICS GP motor type: 1AV2131A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 132S, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",1164,"ΤΕΜ",1,"LVM",1,"1LE10011CA134AC4"]
["1LE1001-1CB03-4AA4","SIMOTICS GP motor type: 1AV2130B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) 4-pole * frame size 132S, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box at top",868,"ΤΕΜ",1,"LVM",1,"1LE10011CB034AA4"]
["1LE1001-1DC43-4AB4","SIMOTICS GP motor type: 1AV2164C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 6-pole * frame size 160L, * 11 kW (50 Hz) 12.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2205,"ΤΕΜ",1,"LVM",1,"1LE10011DC434AB4"]
["1LE1003-0DC32-2AC4","SIMOTICS GP motor type: 1AV3083C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency, 6-pole * frame size 80M * 0.55 kW (50 Hz) 0.63 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 2 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",453,"ΤΕΜ",1,"LVM",1,"1LE10030DC322AC4"]
["1LE1003-0EB03-3AB4","SIMOTICS GP motor type: 1AV3090B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 4-pole * frame size 90S * 1.1 kW (50 Hz) 1.27 kW (60 Hz) 60 Hz, P60: IE2 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 3, MOTOR PROTECTION WITH 1 PTC THERMISTORS FOR SHUTDOWN Terminal box at top",462,"ΤΕΜ",1,"LVM",1,"1LE10030EB033AB4"]
["1LE1003-0EC42-2FB4","SIMOTICS GP motor type: 1AV3094C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 90L * 1.1 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF165 (A200) 1 PTC thermistor for disconnection (2 terminals) Terminal box at top",563,"ΤΕΜ",1,"LVM",1,"1LE10030EC422FB4"]
["1LE1003-1AC43-4FA4","SIMOTICS GP motor type: 1AV3104C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 100L * 1.5 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF215 (A250) without motor protection Terminal box at top",595,"ΤΕΜ",1,"LVM",1,"1LE10031AC434FA4"]
["1LE1003-1BB23-3AA4","SIMOTICS GP motor type: 1AV3112B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 4-pole * frame size 112M, * 4 kW (50 Hz) 4.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B3 Without motor protection Terminal box at top",819,"ΤΕΜ",1,"LVM",1,"1LE10031BB233AA4"]
["1LE1003-1CA00-4FA5","SIMOTICS GP motor type: 1AV3130A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 2-pole * frame size 132S, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF265 (A300) Without motor protection Terminal box on RHS",1036,"ΤΕΜ",1,"LVM",1,"1LE10031CA004FA5"]
["1LE1003-1CB20-4WB6","SIMOTICS GP motor type: 1AV3132B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 132M, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF265 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1492,"ΤΕΜ",1,"LVM",1,"1LE10031CB204WB6"]
["1LE1003-1CC03-4JB5","SIMOTICS GP motor type: 1AV3130C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 132S, * 3 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",1100,"ΤΕΜ",1,"LVM",1,"1LE10031CC034JB5"]
["1LE1003-1CC23-4GC4","SIMOTICS GP motor type: 1AV3132C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 132M, * 4 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",1289,"ΤΕΜ",1,"LVM",1,"1LE10031CC234GC4"]
["1LE1003-1CD03-4JA6","SIMOTICS GP motor type: 1AV3130D low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 8-pole * frame size 132S, * 2.2 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF265 (A300) without motor protection Terminal box on left-hand side",1482,"ΤΕΜ",1,"LVM",1,"1LE10031CD034JA6"]
["1LE1003-1DA33-4AA4","SIMOTICS GP motor type: 1AV3163A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 2-pole * frame size 160M, * 15 kW (50 Hz) 17.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 Without motor protection Terminal box at top",2097,"ΤΕΜ",1,"LVM",1,"1LE10031DA334AA4"]
["1LE1003-1DB20-4WB6","SIMOTICS GP motor type: 1AV3162B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 4-pole * frame size 160M, * 11 kW (50 Hz) 12.6 kW (60 Hz) 60 Hz, P60: IE2 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF300 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",1922,"ΤΕΜ",1,"LVM",1,"1LE10031DB204WB6"]
["1LE1003-1DC22-1AA7","SIMOTICS GP motor type: 1AV3162C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 160M, * 7.5 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B3 without motor protection Terminal box below",1846,"ΤΕΜ",1,"LVM",1,"1LE10031DC221AA7"]
["1LE1003-1DC43-3JB7","SIMOTICS GP motor type: 1AV3164C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 160L, * 11 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 35 * Flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box below",2687,"ΤΕΜ",1,"LVM",1,"1LE10031DC433JB7"]
["1LE1003-1DD32-3AA4","SIMOTICS GP motor type: 1AV3163D low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 8-pole * frame size 160M, * 5.5 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 240 VD/415 VY 3 AC 60 Hz 480 VY IM B3 without motor protection Terminal box at top",2455,"ΤΕΜ",1,"LVM",1,"1LE10031DD323AA4"]
["1LE1003-1EA26-1AA4","SIMOTICS GP motor type: 1AV3182A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 2-pole * frame size 180 * 22 kW (50 Hz) 24.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 230 VYY * 60 Hz 460 VY * 9 main terminals electrical according to NEMA IM B3 without motor protection Terminal box at top",2882,"ΤΕΜ",1,"LVM",1,"1LE10031EA261AA4"]
["1LE1003-1EC42-2GB5","SIMOTICS GP motor type: 1AV3184C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 180 * 15 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",3322,"ΤΕΜ",1,"LVM",1,"1LE10031EC422GB5"]
["1LE1003-2AA42-2GB6","SIMOTICS GP motor type: 1AV3204A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 2-pole * frame size 200 * 30 kW (50 Hz) 33.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",4056,"ΤΕΜ",1,"LVM",1,"1LE10032AA422GB6"]
["1LE1003-2AA53-1JA4","SIMOTICS GP motor type: 1AV3205A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 2-pole * frame size 200 * 37 kW (50 Hz) 41.5 kW (60 Hz) 60 Hz, P60: IE2 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60Hz 400VD/690VY IM B 35 * Flange: FF350 (A400) without motor protection Terminal box at top",4862,"ΤΕΜ",1,"LVM",1,"1LE10032AA531JA4"]
["1LE1003-2AB52-2JC4","SIMOTICS GP motor type: 1AV3205B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 200 * 30 kW (50 Hz) 34.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF350 (A400) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",4035,"ΤΕΜ",1,"LVM",1,"1LE10032AB522JC4"]
["1LE1003-2AC42-1JA6","SIMOTICS GP motor type: 1AV3204C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3, 6-pole * frame size 200 * 18.5 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF350 (A400) without motor protection Terminal box on left-hand side",4017,"ΤΕΜ",1,"LVM",1,"1LE10032AC421JA6"]
["1LE1004-1AA40-4AA6","SIMOTICS GP motor type: 1AV4104A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 2-pole * frame size 100L * 3 kW (50 Hz) 3.45 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box on left-hand side",793,"ΤΕΜ",1,"LVM",1,"1LE10041AA404AA6"]
["1LE1004-1AB40-4JA6","SIMOTICS GP motor type: 1AV4104B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 4-pole * frame size 100L * 2.2 kW (50 Hz) 2.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF215 (A250) without motor protection Terminal box on left-hand side",782,"ΤΕΜ",1,"LVM",1,"1LE10041AB404JA6"]
["1LE1004-1AB43-4JB5","SIMOTICS GP motor type: 1AV4104B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 4-pole * frame size 100L * 2.2 kW (50 Hz) 2.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",843,"ΤΕΜ",1,"LVM",1,"1LE10041AB434JB5"]
["1LE1004-1AB53-3AA4","SIMOTICS GP motor type: 1AV4105B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 4-pole * frame size 100L * 3 kW (50 Hz) 3.45 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 3, without motor protection Terminal box at top",808,"ΤΕΜ",1,"LVM",1,"1LE10041AB533AA4"]
["1LE1004-1BA22-1GA7","SIMOTICS GP motor type: 1AV4112A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 2-pole * frame size 112M, * 4 kW (50 Hz) 4.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF215 (A250) without motor protection Terminal box below",1017,"ΤΕΜ",1,"LVM",1,"1LE10041BA221GA7"]
["1LE1004-1BB20-4GB4","SIMOTICS GP motor type: 1AV4112B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 4-pole * frame size 112M, * 4 kW (50 Hz) 4.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1069,"ΤΕΜ",1,"LVM",1,"1LE10041BB204GB4"]
["1LE1004-1BB22-1JA5","SIMOTICS GP motor type: 1AV4112B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 4-pole * frame size 112M, * 4 kW (50 Hz) 4.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF215 (A250) without motor protection Terminal box on RHS",1105,"ΤΕΜ",1,"LVM",1,"1LE10041BB221JA5"]
["1LE1004-1CA03-4FA6","SIMOTICS GP motor type: 1AV4130A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 2-pole * frame size 132S, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF265 (A300) without motor protection Terminal box on left-hand side",1232,"ΤΕΜ",1,"LVM",1,"1LE10041CA034FA6"]
["1LE1004-1CA12-1GB4","SIMOTICS GP motor type: 1AV4131A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 2-pole * frame size 132S, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1599,"ΤΕΜ",1,"LVM",1,"1LE10041CA121GB4"]
["1LE1004-1CA13-4JC5","SIMOTICS GP motor type: 1AV4131A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 2-pole * frame size 132S, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",1670,"ΤΕΜ",1,"LVM",1,"1LE10041CA134JC5"]
["1LE1004-1CB20-4GA6","SIMOTICS GP motor type: 1AV4132B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 4-pole * frame size 132M, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF265 (A300) without motor protection Terminal box on left-hand side",1640,"ΤΕΜ",1,"LVM",1,"1LE10041CB204GA6"]
["1LE1004-1CB22-2AB4","SIMOTICS GP motor type: 1AV4132B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 4-pole * frame size 132M, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1601,"ΤΕΜ",1,"LVM",1,"1LE10041CB222AB4"]
["1LE1004-1DA22-1AB7","SIMOTICS GP motor type: 1AV4162A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 2-pole * frame size 160M, * 11 kW (50 Hz) 12.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box below",2156,"ΤΕΜ",1,"LVM",1,"1LE10041DA221AB7"]
["1LE1004-1DA32-1JB6","SIMOTICS GP motor type: 1AV4163A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 2-pole * frame size 160M, * 15 kW (50 Hz) 17.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",2842,"ΤΕΜ",1,"LVM",1,"1LE10041DA321JB6"]
["1LE1004-1DA33-4WB7","SIMOTICS GP motor type: 1AV4163A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 2-pole * frame size 160M, * 15 kW (50 Hz) 17.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF300 3 PTC thermistors for disconnection (2 terminals) Terminal box below",2816,"ΤΕΜ",1,"LVM",1,"1LE10041DA334WB7"]
["1LE1004-1DA43-3WB7","SIMOTICS GP motor type: 1AV4164A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 2-pole * frame size 160L, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM V 15 * Flange: FF300 3 PTC thermistors for disconnection (2 terminals) Terminal box below",3359,"ΤΕΜ",1,"LVM",1,"1LE10041DA433WB7"]
["1LE1004-1DA43-4JB4","SIMOTICS GP motor type: 1AV4164A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 2-pole * frame size 160L, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",3212,"ΤΕΜ",1,"LVM",1,"1LE10041DA434JB4"]
["1LE1004-1DB42-2FC4","SIMOTICS GP motor type: 1AV4164B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 4-pole * frame size 160L, * 15 kW (50 Hz) 17.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",2796,"ΤΕΜ",1,"LVM",1,"1LE10041DB422FC4"]
["1LE1004-1DB43-4FB6","SIMOTICS GP motor type: 1AV4164B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Super Premium Efficiency IE4, 4-pole * frame size 160L, * 15 kW (50 Hz) 17.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",2816,"ΤΕΜ",1,"LVM",1,"1LE10041DB434FB6"]
["1LE1012-1CQ23-4AB4","SIMOTICS GP motor type: 1AV1132Q low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure for driving fans double pole-changing * with two windings 6/4-pole * frame size 132M, * 1.7/5.4 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400V IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1291,"ΤΕΜ",1,"LVM",1,"1LE10121CQ234AB4"]
["1LE1501-1CA13-4GB5","SIMOTICS SD motor type: 1CV2131A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 132S, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",1342,"ΤΕΜ",1,"LVM",1,"1LE15011CA134GB5"]
["1LE1501-1EA22-2JA4","SIMOTICS SD motor type: 1CV2182A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 180M, * 22 kW (50 Hz) 24.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",2875,"ΤΕΜ",1,"LVM",1,"1LE15011EA222JA4"]
["1LE1501-1EB23-3GB5","SIMOTICS SD motor type: 1CV2182B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 180M, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",2829,"ΤΕΜ",1,"LVM",1,"1LE15011EB233GB5"]
["1LE1501-1EB23-4AB6","SIMOTICS SD motor type: 1CV2182B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 180M, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",2617,"ΤΕΜ",1,"LVM",1,"1LE15011EB234AB6"]
["1LE1501-1EC42-2GB6","SIMOTICS SD motor type: 1CV2184C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 6-pole * frame size 180L, * 15 kW (50 Hz) 18 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",3309,"ΤΕΜ",1,"LVM",1,"1LE15011EC422GB6"]
["1LE1501-2AA42-1AB4","SIMOTICS SD motor type: 1CV2204A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 200L, * 30 kW (50 Hz) 33.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",3721,"ΤΕΜ",1,"LVM",1,"1LE15012AA421AB4"]
["1LE1501-2AA43-4FB4","SIMOTICS SD motor type: 1CV2204A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 200L, * 30 kW (50 Hz) 33.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",3808,"ΤΕΜ",1,"LVM",1,"1LE15012AA434FB4"]
["1LE1501-2AA52-2WC6","SIMOTICS SD motor type: 1CV2205A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 200L, * 37 kW (50 Hz) 41.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 15 * Flange: FF350 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",5106,"ΤΕΜ",1,"LVM",1,"1LE15012AA522WC6"]
["1LE1501-2AB53-3WB6","SIMOTICS SD motor type: 1CV2205B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 200L, * 30 kW (50 Hz) 34.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 15 * Flange: FF350 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",4145,"ΤΕΜ",1,"LVM",1,"1LE15012AB533WB6"]
["1LE1501-2AC43-4JC5","SIMOTICS SD motor type: 1CV2204C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, 60 Hz, P60: IE1 in EEA: minimum efficiency according to applicable statutory regulations to be considered 6-pole * frame size 200L, * 18.5 kW (50 Hz) 22 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF350 (A400) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",4148,"ΤΕΜ",1,"LVM",1,"1LE15012AC434JC5"]
["1LE1501-2AC53-4AA5","SIMOTICS SD motor type: 1CV2205C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, 60 Hz, P60: IE1 in EEA: minimum efficiency according to applicable statutory regulations to be considered 6-pole * frame size 200L, * 22 kW (50 Hz) 26.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box on RHS",4262,"ΤΕΜ",1,"LVM",1,"1LE15012AC534AA5"]
["1LE1501-2BB02-1JB6","SIMOTICS SD motor type: 1CV2220B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 225S * 37 kW (50 Hz) 42.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF400 (A450) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",4885,"ΤΕΜ",1,"LVM",1,"1LE15012BB021JB6"]
["1LE1501-2BB23-3AA5","SIMOTICS SD motor type: 1CV2222B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 225M * 45 kW (50 Hz) 52 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, without motor protection Terminal box on RHS",5166,"ΤΕΜ",1,"LVM",1,"1LE15012BB233AA5"]
["1LE1501-2BC20-4JA6","SIMOTICS SD motor type: 1CV2222C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, 60 Hz, P60: IE1 in EEA: minimum efficiency according to applicable statutory regulations to be considered 6-pole * frame size 225M * 30 kW (50 Hz) 36 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF400 (A450) without motor protection Terminal box on left-hand side",5755,"ΤΕΜ",1,"LVM",1,"1LE15012BC204JA6"]
["1LE1501-2CA23-3WB6","SIMOTICS SD motor type: 1CV2252A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 250M * 55 kW (50 Hz) 62 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 15 * Flange: FF500 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",7192,"ΤΕΜ",1,"LVM",1,"1LE15012CA233WB6"]
["1LE1501-2CB22-2GB6","SIMOTICS SD motor type: 1CV2252B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 250M * 55 kW (50 Hz) 63 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",6624,"ΤΕΜ",1,"LVM",1,"1LE15012CB222GB6"]
["1LE1501-2CC22-1GA5","SIMOTICS SD motor type: 1CV2252C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, 60 Hz, P60: IE1 in EEA: minimum efficiency according to applicable statutory regulations to be considered 6-pole * frame size 250M * 37 kW (50 Hz) 44.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF500 (A550) without motor protection Terminal box on RHS",7104,"ΤΕΜ",1,"LVM",1,"1LE15012CC221GA5"]
["1LE1501-2DA02-1GB6","SIMOTICS SD motor type: 1CV2280A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 280S, * 75 kW (50 Hz) 84 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",9500,"ΤΕΜ",1,"LVM",1,"1LE15012DA021GB6"]
["1LE1501-2DA22-2GB5","SIMOTICS SD motor type: 1CV2282A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 280M * 90 kW (50 Hz) 101 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",10846,"ΤΕΜ",1,"LVM",1,"1LE15012DA222GB5"]
["1LE1501-2DB03-4WB5","SIMOTICS SD motor type: 1CV2280B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 280S, * 75 kW (50 Hz) 86 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF500 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",9079,"ΤΕΜ",1,"LVM",1,"1LE15012DB034WB5"]
["1LE1501-2DB23-4GC4","SIMOTICS SD motor type: 1CV2282B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 280M * 90 kW (50 Hz) 104 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF500 (A550) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",9861,"ΤΕΜ",1,"LVM",1,"1LE15012DB234GC4"]
["1LE1501-2DC03-4FA5","SIMOTICS SD motor type: 1CV2280C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, 60 Hz, P60: IE1 in EEA: minimum efficiency according to applicable statutory regulations to be considered 6-pole * frame size 280S, * 45 kW (50 Hz) 54 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF500 (A550) without motor protection Terminal box on RHS",8548,"ΤΕΜ",1,"LVM",1,"1LE15012DC034FA5"]
["1LE1501-2DC23-4AC6","SIMOTICS SD motor type: 1CV2282C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, 60 Hz, P60: IE1 in EEA: minimum efficiency according to applicable statutory regulations to be considered 6-pole * frame size 280M * 55 kW (50 Hz) 66 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",9924,"ΤΕΜ",1,"LVM",1,"1LE15012DC234AC6"]
["1LE1501-3AA23-3AB6","SIMOTICS SD motor type: 1CV2312A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 315M, * 132 kW (50 Hz) 148 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",15016,"ΤΕΜ",1,"LVM",1,"1LE15013AA233AB6"]
["1LE1501-3AA42-2GB5","SIMOTICS SD motor type: 1CV2314A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 315L, * 160 kW (50 Hz) 180 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",19022,"ΤΕΜ",1,"LVM",1,"1LE15013AA422GB5"]
["1LE1501-3AB03-3GA4","SIMOTICS SD motor type: 1CV2310B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 315S, * 110 kW (50 Hz) 127 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, Flange: FF600 (A660) without motor protection Terminal box at top",12181,"ΤΕΜ",1,"LVM",1,"1LE15013AB033GA4"]
["1LE1501-3AB43-5JA5","SIMOTICS SD motor type: 1CV2314B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 315L, * 160 kW (50 Hz) 184 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 35 * Flange: FF600 (A660) without motor protection Terminal box on RHS",17670,"ΤΕΜ",1,"LVM",1,"1LE15013AB435JA5"]
["1LE1501-3AC02-1GB6","SIMOTICS SD motor type: 1CV2310C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, 60 Hz, P60: IE1 in EEA: minimum efficiency according to applicable statutory regulations to be considered 6-pole * frame size 315S, * 75 kW (50 Hz) 90 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM V 1 without canopy, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",14004,"ΤΕΜ",1,"LVM",1,"1LE15013AC021GB6"]
["1LE1501-3AC23-3FB5","SIMOTICS SD motor type: 1CV2312C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, 60 Hz, P60: IE1 in EEA: minimum efficiency according to applicable statutory regulations to be considered 6-pole * frame size 315M, * 90 kW (50 Hz) 108 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 5, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",15563,"ΤΕΜ",1,"LVM",1,"1LE15013AC233FB5"]
["1LE1501-3AC53-4AB6","SIMOTICS SD motor type: 1CV2315C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 6-pole * frame size 315L, * 132 kW (50 Hz) 158 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",20898,"ΤΕΜ",1,"LVM",1,"1LE15013AC534AB6"]
["1LE1503-0CB33-3JB4","SIMOTICS SD motor type: 1CV3073B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 4-pole * frame size 71M * 0.37 kW (50 Hz) 0.43 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY 3 AC 60 Hz 440 VD IM B 35 * Flange: FF130 (A160) 1 PTC thermistor for disconnection (2 terminals) Terminal box at top",451,"ΤΕΜ",1,"LVM",1,"1LE15030CB333JB4"]
["1LE1503-0DA32-1JB6","SIMOTICS SD motor type: 1CV3083A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 80M * 1.1 kW (50 Hz) 1.27 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF165 (A200) 1 PTC thermistor for disconnection (2 terminals) Terminal box on left-hand side",576,"ΤΕΜ",1,"LVM",1,"1LE15030DA321JB6"]
["1LE1503-0EA02-2AA5","SIMOTICS SD motor type: 1CV3090A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 90S * 1.5 kW (50 Hz) 1.75 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, without motor protection Terminal box on RHS",591,"ΤΕΜ",1,"LVM",1,"1LE15030EA022AA5"]
["1LE1503-0EB41-7AA4","SIMOTICS SD motor type: 1CV3094B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 4-pole * frame size 90L * 1.5 kW (50 Hz) 1.75 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 220 VD/380 VY IM B 3, without motor protection Terminal box at top",627,"ΤΕΜ",1,"LVM",1,"1LE15030EB417AA4"]
["1LE1503-1AA40-4JA6","SIMOTICS SD motor type: 1CV3104A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * frame size 100L * 3 kW (50 Hz) 3.45 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF215 (A250) without motor protection Terminal box on left-hand side",772,"ΤΕΜ",1,"LVM",1,"1LE15031AA404JA6"]
["1LE1503-1AC42-2JA4","SIMOTICS SD motor type: 1CV3104C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 100L * 1.5 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF215 (A250) without motor protection Terminal box at top",640,"ΤΕΜ",1,"LVM",1,"1LE15031AC422JA4"]
["1LE1503-1BA23-4AC7","SIMOTICS SD motor type: 1CV3112A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * frame size 112M, * 4 kW (50 Hz) 4.55 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",956,"ΤΕΜ",1,"LVM",1,"1LE15031BA234AC7"]
["1LE1503-1BC21-7FA4","SIMOTICS SD motor type: 1CV3112C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 112M, * 2.2 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 220 VD/380 VY IM B 5, flange: FF215 (A250) without motor protection Terminal box at top",841,"ΤΕΜ",1,"LVM",1,"1LE15031BC217FA4"]
["1LE1503-1CA03-4AB4","SIMOTICS SD motor type: 1CV3130A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 132S, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1080,"ΤΕΜ",1,"LVM",1,"1LE15031CA034AB4"]
["1LE1503-1CA12-2JC4","SIMOTICS SD motor type: 1CV3131A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 132S, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF265 (A300) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",1479,"ΤΕΜ",1,"LVM",1,"1LE15031CA122JC4"]
["1LE1503-1CB63-0FA4","SIMOTICS SD motor type: 1CV3136B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing, increased power Basic Line Premium Efficiency IE3, 4-pole * frame size 132M, * 11 kW (50 Hz) 12.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 380 VD/660 VY IM B 5, flange: FF265 (A300) without motor protection Terminal box at top",1988,"ΤΕΜ",1,"LVM",1,"1LE15031CB630FA4"]
["1LE1503-1CC33-0AA4","SIMOTICS SD motor type: 1CV3133C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 132M, * 5.5 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 380 VD/660 VY IM B 3, without motor protection Terminal box at top",1520,"ΤΕΜ",1,"LVM",1,"1LE15031CC330AA4"]
["1LE1503-1DA33-4JC5","SIMOTICS SD motor type: 1CV3163A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 160M, * 15 kW (50 Hz) 17.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",2582,"ΤΕΜ",1,"LVM",1,"1LE15031DA334JC5"]
["1LE1503-1DB20-4AA4","SIMOTICS SD motor type: 1CV3162B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 4-pole * frame size 160M, * 11 kW (50 Hz) 12.6 kW (60 Hz) 60 Hz, P60: IE2 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box at top",1787,"ΤΕΜ",1,"LVM",1,"1LE15031DB204AA4"]
["1LE1503-1DC20-4FA4","SIMOTICS SD motor type: 1CV3162C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 160M, * 7.5 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",1948,"ΤΕΜ",1,"LVM",1,"1LE15031DC204FA4"]
["1LE1503-1EA60-2FA4","SIMOTICS SD motor type: 1CV3186A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing, increased power Basic Line Premium Efficiency IE3, 2-pole * frame size 180L, * 30 kW (50 Hz) 33.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",4212,"ΤΕΜ",1,"LVM",1,"1LE15031EA602FA4"]
["1LE1503-1EB42-2JA4","SIMOTICS SD motor type: 1CV3184B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 4-pole * frame size 180L, * 22 kW (50 Hz) 25.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",3114,"ΤΕΜ",1,"LVM",1,"1LE15031EB422JA4"]
["1LE1503-1EC42-1FA5","SIMOTICS SD motor type: 1CV3184C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 180L, * 15 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF300 (A350) without motor protection Terminal box on RHS",3554,"ΤΕΜ",1,"LVM",1,"1LE15031EC421FA5"]
["1LE1503-1EC62-7FA4","SIMOTICS SD motor type: 1CV3186C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing, increased power Basic Line Premium Efficiency IE3, 6-pole * frame size 180L, * 18.5 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 500 VY 3 AC 60Hz 575VY IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",4179,"ΤΕΜ",1,"LVM",1,"1LE15031EC627FA4"]
["1LE1503-2AA43-4FB5","SIMOTICS SD motor type: 1CV3204A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 200L, * 30 kW (50 Hz) 33.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",4400,"ΤΕΜ",1,"LVM",1,"1LE15032AA434FB5"]
["1LE1503-2AB53-0JA4","SIMOTICS SD motor type: 1CV3205B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 200L, * 30 kW (50 Hz) 34.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 380 VD/660 VY IM B 35 * Flange: FF350 (A400) without motor protection Terminal box at top",4117,"ΤΕΜ",1,"LVM",1,"1LE15032AB530JA4"]
["1LE1503-2AC42-2FC6","SIMOTICS SD motor type: 1CV3204C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 200L, * 18.5 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF350 (A400) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",4464,"ΤΕΜ",1,"LVM",1,"1LE15032AC422FC6"]
["1LE1503-2AC63-5JA4","SIMOTICS SD motor type: 1CV3206C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing, increased power Basic Line Premium Efficiency IE3, 6-pole * frame size 200L, * 30 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 35 * Flange: FF350 (A400) without motor protection Terminal box at top",6376,"ΤΕΜ",1,"LVM",1,"1LE15032AC635JA4"]
["1LE1503-2BA63-3JA4","SIMOTICS SD motor type: 1CV3226A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing, increased power Basic Line Premium Efficiency IE3, 2-pole * frame size 225M * 55 kW (50 Hz) 62 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF400 (A450) without motor protection Terminal box at top",7281,"ΤΕΜ",1,"LVM",1,"1LE15032BA633JA4"]
["1LE1503-2BB20-4AA5","SIMOTICS SD motor type: 1CV3222B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 225M * 45 kW (50 Hz) 52 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, without motor protection Terminal box on RHS",5424,"ΤΕΜ",1,"LVM",1,"1LE15032BB204AA5"]
["1LE1503-2BB63-4AB4","SIMOTICS SD motor type: 1CV3226B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing, increased power Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 225M * 55 kW (50 Hz) 63 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",6682,"ΤΕΜ",1,"LVM",1,"1LE15032BB634AB4"]
["1LE1503-2BC23-3AB5","SIMOTICS SD motor type: 1CV3222C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 225M * 30 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",6180,"ΤΕΜ",1,"LVM",1,"1LE15032BC233AB5"]
["1LE1503-2CB23-3FB5","SIMOTICS SD motor type: 1CV3252B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 250M * 55 kW (50 Hz) 63 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 5, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",7164,"ΤΕΜ",1,"LVM",1,"1LE15032CB233FB5"]
["1LE1503-2CC22-1FA4","SIMOTICS SD motor type: 1CV3252C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 250M * 37 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 5, flange: FF500 (A550) without motor protection Terminal box at top",7324,"ΤΕΜ",1,"LVM",1,"1LE15032CC221FA4"]
["1LE1503-2CC63-3FA4","SIMOTICS SD motor type: 1CV3256C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing, increased power Basic Line Premium Efficiency IE3, 6-pole * frame size 250M * 45 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 5, flange: FF500 (A550) without motor protection Terminal box at top",9203,"ΤΕΜ",1,"LVM",1,"1LE15032CC633FA4"]
["1LE1503-2DA22-1AA4","SIMOTICS SD motor type: 1CV3282A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * frame size 280M * 90 kW (50 Hz) 101 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, without motor protection Terminal box at top",10589,"ΤΕΜ",1,"LVM",1,"1LE15032DA221AA4"]
["1LE1503-2DB22-2AA4","SIMOTICS SD motor type: 1CV3282B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 280M * 90 kW (50 Hz) 104 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, without motor protection Terminal box at top",9798,"ΤΕΜ",1,"LVM",1,"1LE15032DB222AA4"]
["1LE1503-2DC20-4WB5","SIMOTICS SD motor type: 1CV3282C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 280M * 55 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF500 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",11111,"ΤΕΜ",1,"LVM",1,"1LE15032DC204WB5"]
["1LE1503-2DC23-4AB4","SIMOTICS SD motor type: 1CV3282C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 280M * 55 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",10010,"ΤΕΜ",1,"LVM",1,"1LE15032DC234AB4"]
["1LE1503-3AA23-3GA5","SIMOTICS SD motor type: 1CV3312A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 315M, * 132 kW (50 Hz) 148 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, Flange: FF600 (A660) without motor protection Terminal box on RHS",16294,"ΤΕΜ",1,"LVM",1,"1LE15033AA233GA5"]
["1LE1503-3AA53-3GA5","SIMOTICS SD motor type: 1CV3315A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 315L, * 200 kW (50 Hz) 224 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, Flange: FF600 (A660) without motor protection Terminal box on RHS",24758,"ΤΕΜ",1,"LVM",1,"1LE15033AA533GA5"]
["1LE1503-3AB03-3JB5","SIMOTICS SD motor type: 1CV3310B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 4-pole * frame size 315S, * 110 kW (50 Hz) 127 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",13817,"ΤΕΜ",1,"LVM",1,"1LE15033AB033JB5"]
["1LE1503-3AB42-1JA6","SIMOTICS SD motor type: 1CV3314B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 4-pole * frame size 315L, * 160 kW (50 Hz) 184 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF600 (A660) without motor protection Terminal box on left-hand side",18869,"ΤΕΜ",1,"LVM",1,"1LE15033AB421JA6"]
["1LE1503-3AC43-4JA5","SIMOTICS SD motor type: 1CV3314C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 315L, * 110 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF600 (A660) without motor protection Terminal box on RHS",19228,"ΤΕΜ",1,"LVM",1,"1LE15033AC434JA5"]
["1LE1503-3AC62-2AA4","SIMOTICS SD motor type: 1CV3316C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 315L, * 160 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, without motor protection Terminal box at top",27361,"ΤΕΜ",1,"LVM",1,"1LE15033AC622AA4"]
["1LE1504-1AB51-7FA4","SIMOTICS SD motor type: 1CV4105B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 4-pole * frame size 100L * 3 kW (50 Hz) 3.45 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 220 VD/380 VY IM B 5, flange: FF215 (A250) without motor protection Terminal box at top",918,"ΤΕΜ",1,"LVM",1,"1LE15041AB517FA4"]
["1LE1504-1CA13-4GB4","SIMOTICS SD motor type: 1CV4131A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 2-pole * frame size 132S, * 7.5 kW (50 Hz) 8.6 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1686,"ΤΕΜ",1,"LVM",1,"1LE15041CA134GB4"]
["1LE1504-1CB03-4JA4","SIMOTICS SD motor type: 1CV4130B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 4-pole * frame size 132S, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF265 (A300) without motor protection Terminal box at top",1362,"ΤΕΜ",1,"LVM",1,"1LE15041CB034JA4"]
["1LE1504-1DA43-5JA4","SIMOTICS SD motor type: 1CV4164A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 2-pole * frame size 160L, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 415VD * 3 AC 60 Hz 480 VD IM B 35 * Flange: FF300 (A350) without motor protection Terminal box at top",3420,"ΤΕΜ",1,"LVM",1,"1LE15041DA435JA4"]
["1LE1504-1EB22-2FA4","SIMOTICS SD motor type: 1CV4182B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 4-pole * frame size 180M, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF300 (A350) without motor protection Terminal box at top",3216,"ΤΕΜ",1,"LVM",1,"1LE15041EB222FA4"]
["1LE1504-1EB43-3WB6","SIMOTICS SD motor type: 1CV4184B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 4-pole * frame size 180L, * 22 kW (50 Hz) 25.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 15 * Flange: FF300 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",4124,"ΤΕΜ",1,"LVM",1,"1LE15041EB433WB6"]
["1LE1504-2AA52-2JA4","SIMOTICS SD motor type: 1CV4205A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 2-pole * frame size 200L, * 37 kW (50 Hz) 41.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF350 (A400) without motor protection Terminal box at top",6004,"ΤΕΜ",1,"LVM",1,"1LE15042AA522JA4"]
["1LE1504-2AB51-8JA4","SIMOTICS SD motor type: 1CV4205B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 4-pole * frame size 200L, * 30 kW (50 Hz) 34.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 60 Hz 230 VD/400 VY IM B 35 * Flange: FF350 (A400) without motor protection Terminal box at top",4868,"ΤΕΜ",1,"LVM",1,"1LE15042AB518JA4"]
["1LE1504-2BB20-4WB6","SIMOTICS SD motor type: 1CV4222B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 60 Hz, P60: IE3 4-pole * frame size 225M * 45 kW (50 Hz) 52 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF400 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",6748,"ΤΕΜ",1,"LVM",1,"1LE15042BB204WB6"]
["1LE1504-2BB23-4WC5","SIMOTICS SD motor type: 1CV4222B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 60 Hz, P60: IE3 4-pole * frame size 225M * 45 kW (50 Hz) 52 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 15 * Flange: FF400 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on RHS",6865,"ΤΕΜ",1,"LVM",1,"1LE15042BB234WC5"]
["1LE1504-2CB22-2FA4","SIMOTICS SD motor type: 1CV4252B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 4-pole * frame size 250M * 55 kW (50 Hz) 63 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, flange: FF500 (A550) without motor protection Terminal box at top",7457,"ΤΕΜ",1,"LVM",1,"1LE15042CB222FA4"]
["1LE1504-2DA03-4AB6","SIMOTICS SD motor type: 1CV4280A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 2-pole * frame size 280S, * 75 kW (50 Hz) 84 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",10877,"ΤΕΜ",1,"LVM",1,"1LE15042DA034AB6"]
["1LE1504-2DB02-2GB6","SIMOTICS SD motor type: 1CV4280B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 4-pole * frame size 280S, * 75 kW (50 Hz) 86 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",10690,"ΤΕΜ",1,"LVM",1,"1LE15042DB022GB6"]
["1LE1504-3AA02-1AA6","SIMOTICS SD motor type: 1CV4310A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 2-pole * frame size 315S, * 110 kW (50 Hz) 123 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, without motor protection Terminal box on left-hand side",14908,"ΤΕΜ",1,"LVM",1,"1LE15043AA021AA6"]
["1LE1504-3AA03-3FA4","SIMOTICS SD motor type: 1CV4310A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 2-pole * frame size 315S, * 110 kW (50 Hz) 123 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM B 5, Flange: FF600 (A660) without motor protection Terminal box at top",14938,"ΤΕΜ",1,"LVM",1,"1LE15043AA033FA4"]
["1LE1504-3AA43-3GA6","SIMOTICS SD motor type: 1CV4314A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 2-pole * frame size 315L, * 160 kW (50 Hz) 180 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, Flange: FF600 (A660) without motor protection Terminal box on left-hand side",22673,"ΤΕΜ",1,"LVM",1,"1LE15043AA433GA6"]
["1LE1504-3AA53-4GC4","SIMOTICS SD motor type: 1CV4315A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 2-pole * frame size 315L, * 200 kW (50 Hz) 224 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, Flange: FF600 (A660) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",27507,"ΤΕΜ",1,"LVM",1,"1LE15043AA534GC4"]
["1LE1504-3AB02-2FB4","SIMOTICS SD motor type: 1CV4310B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 4-pole * frame size 315M, * 110 kW (50 Hz) 127 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 5, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",14622,"ΤΕΜ",1,"LVM",1,"1LE15043AB022FB4"]
["1LE1504-3AB22-2AC4","SIMOTICS SD motor type: 1CV4312B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 4-pole * frame size 315M, * 132 kW (50 Hz) 152 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",16614,"ΤΕΜ",1,"LVM",1,"1LE15043AB222AC4"]
["1LE1504-3AB42-7AA4","SIMOTICS SD motor type: 1CV4314B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Super Premium Efficiency IE4, 4-pole * frame size 315L, * 160 kW (50 Hz) 184 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 500 VY 3 AC 60Hz 575VY IM B 3, without motor protection Terminal box at top",19700,"ΤΕΜ",1,"LVM",1,"1LE15043AB427AA4"]
["1LE1601-1CB03-4FB4","SIMOTICS SD motor type: 1CV2130B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line in EEA: minimum efficiency acc. to applicable statutory regulations to be considered! (as of 01.01.2017) High Efficiency IE2, 4-pole * frame size 132S, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 5, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1107,"ΤΕΜ",1,"LVM",1,"1LE16011CB034FB4"]
["1LE1601-1EB23-4JC4","SIMOTICS SD motor type: 1CV2182B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 180M, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",2912,"ΤΕΜ",1,"LVM",1,"1LE16011EB234JC4"]
["1LE1601-2AA42-2JC6","SIMOTICS SD motor type: 1CV2204A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 200L, * 30 kW (50 Hz) 33.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF350 (A400) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",4528,"ΤΕΜ",1,"LVM",1,"1LE16012AA422JC6"]
["1LE1601-2AC50-4JB6","SIMOTICS SD motor type: 1CV2205C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line High Efficiency IE2, 60 Hz, P60: IE1 in EEA: minimum efficiency according to applicable statutory regulations to be considered 6-pole * frame size 200L, * 22 kW (50 Hz) 26.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",4882,"ΤΕΜ",1,"LVM",1,"1LE16012AC504JB6"]
["1LE1601-2BB02-1AB5","SIMOTICS SD motor type: 1CV2220B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 225S * 37 kW (50 Hz) 42.5 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",4848,"ΤΕΜ",1,"LVM",1,"1LE16012BB021AB5"]
["1LE1601-2CA23-4AB6","SIMOTICS SD motor type: 1CV2252A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 250M * 55 kW (50 Hz) 62 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",7124,"ΤΕΜ",1,"LVM",1,"1LE16012CA234AB6"]
["1LE1601-2DA02-2AB4","SIMOTICS SD motor type: 1CV2280A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 280S, * 75 kW (50 Hz) 84 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",8495,"ΤΕΜ",1,"LVM",1,"1LE16012DA022AB4"]
["1LE1601-2DB02-2GC6","SIMOTICS SD motor type: 1CV2280B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 280S, * 75 kW (50 Hz) 86 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF500 (A550) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",9217,"ΤΕΜ",1,"LVM",1,"1LE16012DB022GC6"]
["1LE1601-2DB23-3GB4","SIMOTICS SD motor type: 1CV2282B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 280M * 90 kW (50 Hz) 104 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",10037,"ΤΕΜ",1,"LVM",1,"1LE16012DB233GB4"]
["1LE1601-3AA02-1JB4","SIMOTICS SD motor type: 1CV2310A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 2-pole * frame size 315S, * 110 kW (50 Hz) 123 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",13244,"ΤΕΜ",1,"LVM",1,"1LE16013AA021JB4"]
["1LE1601-3AB02-2AC4","SIMOTICS SD motor type: 1CV2310B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 315S, * 110 kW (50 Hz) 127 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 3, 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box at top",12080,"ΤΕΜ",1,"LVM",1,"1LE16013AB022AC4"]
["1LE1601-3AB43-3GB5","SIMOTICS SD motor type: 1CV2314B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line High Efficiency IE2, in EEA: minimum efficiency according to applicable statutory regulations to be considered! 4-pole * frame size 315L, * 160 kW (50 Hz) 184 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",18119,"ΤΕΜ",1,"LVM",1,"1LE16013AB433GB5"]
["1LE1601-3AC42-2JB4","SIMOTICS SD motor type: 1CV2314C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line High Efficiency IE2, 60 Hz, P60: IE1 in EEA: minimum efficiency according to applicable statutory regulations to be considered 6-pole * frame size 315L, * 110 kW (50 Hz) 132 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",18085,"ΤΕΜ",1,"LVM",1,"1LE16013AC422JB4"]
["1LE1603-1AA42-2GC7","SIMOTICS SD motor type: 1CV3104A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line Premium Efficiency IE3, 60 Hz, P60: IE2 2-pole * frame size 100L * 3 kW (50 Hz) 3.45 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF215 (A250) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",947,"ΤΕΜ",1,"LVM",1,"1LE16031AA422GC7"]
["1LE1603-1CA02-1AB5","SIMOTICS SD motor type: 1CV3130A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line Premium Efficiency IE3, 2-pole * frame size 132S, * 5.5 kW (50 Hz) 6.3 kW (60 Hz) 60 Hz, P60: IE2 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 220 VD/380 VY 3 AC 60 Hz 440 VY IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",1223,"ΤΕΜ",1,"LVM",1,"1LE16031CA021AB5"]
["1LE1603-1DA22-2JC7","SIMOTICS SD motor type: 1CV3162A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line Premium Efficiency IE3, 2-pole * frame size 160M, * 11 kW (50 Hz) 12.6 kW (60 Hz) 60 Hz, P60: IE2 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF300 (A350) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box below",2272,"ΤΕΜ",1,"LVM",1,"1LE16031DA222JC7"]
["1LE1603-1DA42-2GB5","SIMOTICS SD motor type: 1CV3164A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line Premium Efficiency IE3, 2-pole * frame size 160L, * 18.5 kW (50 Hz) 21.3 kW (60 Hz) 60 Hz, P60: IE2 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",3215,"ΤΕΜ",1,"LVM",1,"1LE16031DA422GB5"]
["1LE1603-1EB42-2GB6","SIMOTICS SD motor type: 1CV3184B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line Premium Efficiency IE3, 4-pole * frame size 180L, * 22 kW (50 Hz) 25.3 kW (60 Hz) 60 Hz, P60: IE2 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",3544,"ΤΕΜ",1,"LVM",1,"1LE16031EB422GB6"]
["1LE1603-1EC43-4GB6","SIMOTICS SD motor type: 1CV3184C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line Premium Efficiency IE3, 6-pole * frame size 180L, * 15 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",3752,"ΤΕΜ",1,"LVM",1,"1LE16031EC434GB6"]
["1LE1603-2AC52-2GB6","SIMOTICS SD motor type: 1CV3205C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line Premium Efficiency IE3, 6-pole * frame size 200L, * 22 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V 1 without canopy, flange: FF350 (A400) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",5244,"ΤΕΜ",1,"LVM",1,"1LE16032AC522GB6"]
["1LE1603-2CB22-2JC6","SIMOTICS SD motor type: 1CV3252B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 250M * 55 kW (50 Hz) 63 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF500 (A550) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",8001,"ΤΕΜ",1,"LVM",1,"1LE16032CB222JC6"]
["1LE1603-2CC23-4AB6","SIMOTICS SD motor type: 1CV3252C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line Premium Efficiency IE3, 6-pole * frame size 250M * 37 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",7853,"ΤΕΜ",1,"LVM",1,"1LE16032CC234AB6"]
["1LE1603-2DC22-2JB6","SIMOTICS SD motor type: 1CV3282C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line Premium Efficiency IE3, 6-pole * frame size 280M * 55 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B 35 * Flange: FF500 (A550) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",11054,"ΤΕΜ",1,"LVM",1,"1LE16032DC222JB6"]
["1LE1603-3AB23-3GB6","SIMOTICS SD motor type: 1CV3312B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line Premium Efficiency IE3, 4-pole * frame size 315M, * 132 kW (50 Hz) 152 kW (60 Hz) 60 Hz, P60: IE2 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 380 VD/660 VY * 3 AC 60 Hz 440 VD IM V 1 without canopy, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",16190,"ΤΕΜ",1,"LVM",1,"1LE16033AB233GB6"]
["1LE1603-3AB53-4GB4","SIMOTICS SD motor type: 1CV3315B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line Premium Efficiency IE3, 60 Hz, P60: IE2 4-pole * frame size 315L, * 200 kW (50 Hz) 230 kW (60 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1 without canopy, Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",22911,"ΤΕΜ",1,"LVM",1,"1LE16033AB534GB4"]
["1LE1603-3AC40-4AB6","SIMOTICS SD motor type: 1CV3314C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line Premium Efficiency IE3, 6-pole * frame size 315L, * 110 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",19071,"ΤΕΜ",1,"LVM",1,"1LE16033AC404AB6"]
["1LE1603-3AC50-4JB6","SIMOTICS SD motor type: 1CV3315C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing performance line Premium Efficiency IE3, 6-pole * frame size 315L, * 132 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50Hz 400VD * 3 AC 60 Hz 460 VD IM B 35 * Flange: FF600 (A660) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",23240,"ΤΕΜ",1,"LVM",1,"1LE16033AC504JB6"]
["1LE5504-3AA73-4GB6","SIMOTICS SD motor type: 1CV4317A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE4 2-pole * frame size 315L* 315 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V 1, Flange: FF740 (A800) 3 PTC thermistors for disconnection (2 terminals) Terminal box on left-hand side",40388,"ΤΕΜ",1,"LVM",1,"1LE55043AA734GB6"]
["1LE5504-3AB73-3FB5","SIMOTICS SD motor type: 1CV4317B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE4 4-pole * frame size 315L* 315 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 5, Flange: FF740 (A800) 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",38148,"ΤΕΜ",1,"LVM",1,"1LE55043AB733FB5"]
["1LE5603-3AB63-4GC6","SIMOTICS SD motor type: 1CV3316B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Performance Line Premium Efficiency IE3, 4-pole * frame size 315L* 250 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1, Flange: FF740 (A800) 6 PTC thermistors for warning and shutdown (4 terminals) Terminal box on left-hand side",28075,"ΤΕΜ",1,"LVM",1,"1LE56033AB634GC6"]
["1LE5603-3BA43-4FB0","SIMOTICS SD motor type: 1CV3354A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Performance Line Premium Efficiency IE3, 2-pole * frame size 355L * 400 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, Flange: FF840 (A900) disconnection (2 terminals) Terminal box base left with terminal box at top",49161,"ΤΕΜ",1,"LVM",1,"1LE56033BA434FB0"]
["1LE5604-3AB63-3AB5","SIMOTICS SD motor type: 1CV4316B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Performance Line Premium Efficiency IE4 4-pole * frame size 315L* 250 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50HZ 380VD/660VY * 3 AC 60HZ 440VD IM B 3, 3 PTC thermistors for disconnection (2 terminals) Terminal box on RHS",30719,"ΤΕΜ",1,"LVM",1,"1LE56043AB633AB5"]
["1LE5604-3BA33-4FB0","SIMOTICS SD motor type: 1CV4353A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Performance Line Premium Efficiency IE4 2-pole * frame size 355L * 355 kW (50 Hz) standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, Flange: FF840 (A900) disconnection (2 terminals) Terminal box base left with terminal box at top",48275,"ΤΕΜ",1,"LVM",1,"1LE56043BA334FB0"]
["1MB1011-1BA23-4AA4","SIMOTICS XP motor type: 1AV2112A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP65 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2 2-pole * size 112M * 4 kW (50 Hz) 4.55 kW (60 Hz) version for zone 21 and zone 22 with conductive dust standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 without motor protection Terminal box at top",821,"ΤΕΜ",1,"LVM",1,"1MB10111BA234AA4"]
["1MB1013-0EA02-2HA4","SIMOTICS XP motor type: 1AV3090A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP65 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3 2-pole * frame size 90S * 1.5 kW (50 Hz) 1.75 kW (60 Hz) version for zone 21 and zone 22 with conductive dust standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V3, flange: FF165 (A200) without motor protection Terminal box at top",590,"ΤΕΜ",1,"LVM",1,"1MB10130EA022HA4"]
["1MB1013-1CA13-4HB4","SIMOTICS XP motor type: 1AV3131A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP65 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3 2-pole * frame size 132S * 7.5 kW (50 Hz) 8.6 kW (60 Hz) version for zone 21 and zone 22 with conductive dust standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V3, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1552,"ΤΕΜ",1,"LVM",1,"1MB10131CA134HB4"]
["1MB1013-1DA23-4AA4","SIMOTICS XP motor type: 1AV3162A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP65 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3 2-pole * frame size 160M * 11 kW (50 Hz) 12.6 kW (60 Hz) version for zone 21 and zone 22 with conductive dust standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 without motor protection Terminal box at top",1919,"ΤΕΜ",1,"LVM",1,"1MB10131DA234AA4"]
["1MB1023-0DA33-4HB4","SIMOTICS XP motor type: 1AV3083A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3 2-pole * frame size 80M * 1.1 kW (50 Hz) 1.27 kW (60 Hz) version for zone 22 for non-conductive dust standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM V3, flange: FF165 (A200) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",480,"ΤΕΜ",1,"LVM",1,"1MB10230DA334HB4"]
["1MB1023-1AC43-4FA4","SIMOTICS XP motor type: 1AV3104C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3 6-pole * frame size 100L * 1.5 kW (50 Hz) 1.75 kW (60 Hz)  60 Hz IE2 version for zone 22 for non-conductive dust standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF215 (A250) without motor protection Terminal box at top",685,"ΤΕΜ",1,"LVM",1,"1MB10231AC434FA4"]
["1MB1023-1CC23-4FA4","SIMOTICS XP motor type: 1AV3132C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3 6-pole * frame size 132M * 4 kW (50 Hz) 4.55 kW (60 Hz), 60 Hz, P60: IE2 version for zone 22 for non-conductive dust standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF265 (A300) without motor protection Terminal box at top",1315,"ΤΕΜ",1,"LVM",1,"1MB10231CC234FA4"]
["1MB1031-1AB52-2HA4","SIMOTICS XP motor type: 1AV2105B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2 4-pole * frame size 100L * 3 kW (50 Hz) 3.45 kW (60 Hz) Ex ec IIC T3 Gc version for zone 2 according to IEC/EN 60 079-7 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V3, flange: FF215 (A250) without motor protection Terminal box at top",745,"ΤΕΜ",1,"LVM",1,"1MB10311AB522HA4"]
["1MB1031-1CC32-2HB4","SIMOTICS XP motor type: 1AV2133C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure High Efficiency IE2 6-pole * frame size 132M * 5.5 kW (50 Hz) 6.3 kW (60 Hz) Ex ec IIC T3 Gc version for zone 2 according to IEC/EN 60 079-7 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V3, flange: FF265 (A300) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1590,"ΤΕΜ",1,"LVM",1,"1MB10311CC322HB4"]
["1MB1033-0EB02-2AB4","SIMOTICS XP motor type: 1AV3090B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3 4-pole * frame size 90S * 1.1 kW (50 Hz) 1.27 kW (60 Hz), 60 Hz, P60: IE2 Ex ec IIC T3 Gc version for zone 2 according to IEC/EN 60 079-7 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",533,"ΤΕΜ",1,"LVM",1,"1MB10330EB022AB4"]
["1MB1033-1CC22-2HA4","SIMOTICS XP motor type: 1AV3132C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) aluminum enclosure Premium Efficiency IE3 6-pole * frame size 132M * 4 kW (50 Hz) 4.55 kW (60 Hz), 60 Hz, P60: IE2 Ex ec IIC T3 Gc version for zone 2 according to IEC/EN 60 079-7 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 230 VD/400 VY * 3 AC 60 Hz 460 VY IM V3, flange: FF265 (A300) without motor protection Terminal box at top",1353,"ΤΕΜ",1,"LVM",1,"1MB10331CC222HA4"]
["1MB1511-1DA42-2HB4","SIMOTICS XP motor type: 1CV2164A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP65 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2 2-pole * frame size 160L * 18.5 kW (50 Hz), 21.3 kW (60 Hz) Ex tb IIIC T120Β° Db version for zone 21 and zone 22 with conductive dust standard color RAL 7030, if no order code is specified for selecting another color. 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM V3, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2959,"ΤΕΜ",1,"LVM",1,"1MB15111DA422HB4"]
["1MB1513-0EB42-2HA4","SIMOTICS XP motor type: 1CV3094B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP65 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 4-pole * frame size 90L * 1.5 kW (50 Hz), 1.75 kW (60 Hz) Ex tb IIIC T120Β° Db version for zone 21 and zone 22 with conductive dust standard color RAL 7030, if no order code is specified for selecting another color. 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM V 3, flange: FF165 (A200) without motor protection Terminal box at top",769,"ΤΕΜ",1,"LVM",1,"1MB15130EB422HA4"]
["1MB1513-1CB02-2FA4","SIMOTICS XP motor type: 1CV3130B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP65 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 4-pole * frame size 132S * 5.5 kW (50 Hz), 6.3 kW (60 Hz) Ex tb IIIC T120Β° Db version for zone 21 and zone 22 with conductive dust standard color RAL 7030, if no order code is specified for selecting another color. 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM B5, flange: FF265 (A300) without motor protection Terminal box at top",1370,"ΤΕΜ",1,"LVM",1,"1MB15131CB022FA4"]
["1MB1513-1DB43-4FB4","SIMOTICS XP motor type: 1CV3164B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP65 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 4-pole * frame size 160L * 15 kw (50 Hz), 17.3 kW (60 Hz), P60: IE2 Ex tb IIIC T120Β° Db version for zone 21 and zone 22 with conductive dust standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2845,"ΤΕΜ",1,"LVM",1,"1MB15131DB434FB4"]
["1MB1523-0EA42-2HB4","SIMOTICS XP motor type: 1CV3094A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 90L * 2.2 kW (50 Hz), 2.55 kW (60 Hz) Ex tc IIIB T120Β° Dc version for zone 22 for non-conductive dust standard color RAL 7030, if no order code is specified for selecting another color. 3AC 50 Hz 230VD/400VY * 3AC 60 Hz 460VY IM V 3, flange: FF165 (A200) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",792,"ΤΕΜ",1,"LVM",1,"1MB15230EA422HB4"]
["1MB1523-1BB23-4FB4","SIMOTICS XP motor type: 1CV3112B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 4-pole * frame size 112M * 4 kW (50 Hz), 4.55 kW (60 Hz) Ex tc IIIB T120Β° Dc version for zone 22 for non-conductive dust standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF215 (A250) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",1091,"ΤΕΜ",1,"LVM",1,"1MB15231BB234FB4"]
["1MB1523-1DA33-4FA4","SIMOTICS XP motor type: 1CV3163A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 160M * 15 kW (50 Hz), 17.3 kW (60 Hz) Ex tc IIIB T120Β° Dc version for zone 22 for non-conductive dust standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF300 (A350) without motor protection Terminal box at top",2635,"ΤΕΜ",1,"LVM",1,"1MB15231DA334FA4"]
["1MB1531-1CB23-4AA4","SIMOTICS XP motor type: 1CV2132B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2 4-pole * frame size 132M * 7.5 kW (50 Hz), 8.6 kW (60 Hz) Ex ec IIC T3 Gc version for zone 2 according to IEC/EN 60 079-7 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 without motor protection Terminal box at top",1419,"ΤΕΜ",1,"LVM",1,"1MB15311CB234AA4"]
["1MB1531-2DC03-4AB4","SIMOTICS XP motor type: 1CV2280C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line High Efficiency IE2 6-pole * frame size 280S * 45 kW (50 Hz), 54 kW (60 Hz), P60:IE1 Ex ec IIC T3 Gc version for zone 2 according to IEC/EN 60 079-7 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B3 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",8913,"ΤΕΜ",1,"LVM",1,"1MB15312DC034AB4"]
["1MB1533-1AB53-4FA4","SIMOTICS XP motor type: 1CV3105B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 4-pole * frame size 100L * 3 kW (50 Hz), 3.45 kW (60 Hz) Ex ec IIC T3 Gc version for zone 2 according to IEC/EN 60 079-7 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF215 (A250) without motor protection Terminal box at top",875,"ΤΕΜ",1,"LVM",1,"1MB15331AB534FA4"]
["1MB1533-1DA23-4FB4","SIMOTICS XP motor type: 1CV3162A low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 2-pole * frame size 160M * 11 kW (50 Hz), 12.6 kW (60 Hz) Ex ec IIC T3 Gc version for zone 2 according to IEC/EN 60 079-7 standard color RAL 7030, if no order code is specified for selecting another color. 3 AC 50 Hz 400 VD/690 VY * 3 AC 60 Hz 460 VD IM B5, flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",2209,"ΤΕΜ",1,"LVM",1,"1MB15331DA234FB4"]
["1MB1553-1DC43-4FB4","SIMOTICS XP motor type: 1CD3164C low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 6-pole * frame size 160L * 11 kW (50 Hz), 11 kW (60 Hz) EX DB (EB) IIC T4 version for zone 1 standard color RAL 7030, if no order code is specified for selecting another color. 3AC 50 Hz 400VD/690VY * 3AC 60 Hz 460VD IM B5, Flange: FF300 (A350) 3 PTC thermistors for disconnection (2 terminals) Terminal box at top",7235,"ΤΕΜ",1,"LVM",1,"1MB15531DC434FB4"]
["1MB1553-2DB03-4FA4","SIMOTICS XP motor type: 1CD3280B low-voltage motor, IEC squirrel-cage rotor, self-cooled, IP55 temperature class 155(F) according to 130(B) gray cast iron housing Basic Line Premium Efficiency IE3, 4-pole * frame size 280S * 75 kW (50 Hz), 75 kW (60 Hz) EX DB (EB) IIC T4 version for zone 1 standard color RAL 7030, if no order code is specified for selecting another color. 3AC 50 Hz 400VD/690VY * 3AC 60 Hz 460VD IM B5, Flange: FF500 (A550) without motor protection Terminal box at top",20394,"ΤΕΜ",1,"LVM",1,"1MB15532DB034FA4"]
["3AX1133-3H","accessory for 3AH,3AK,3AE lubricant KlΓΌber Isoflex Topas L32 180g-tube",138,"ST",1,"LP","On request","3AX11333H"]
["3AX1438-5N","accessory for 3AE5 separating shell width across flats 205mm 7.2 up to 12kV (31.5kA) 17.5kV (25kA) (Fa. Ritter)",232,"ST",1,"LP","On request","3AX14385N"]
["3AX1470-2A","accessory for 3AE1 cover for pole-center distance 210mm (13. digit = 0) Serial number required for label printing",807,"ST",1,"LP","On request","3AX14702A"]
["3AX7111-2G","accessory for 3AE slide-in module PCD 210mm width across flats 310mm <=17.5 kV <=1250A <= 31.5kA",20608,"ST",1,"LP","On request","3AX71112G"]
["3AY1714-0G","spare part for 3AH5 vacuum interrupter as complete pole for 24kV 16kA 800A",7264,"ST",1,"LP","On request","3AY17140G"]
["3CX1025","Operating shaft lever for switch disconnector","On Request",null,null,"LP",1,"3CX1025"]
["3KA5230-1GE01","Switch disconnector in new design Iu=125 A, Ue = 690 V, 3-pole with door drive 8UC7 Handle dark blue/blue-green Basic masking frame light gray",891.81,"ST",1,"LP",1,"3KA52301GE01"]
["3KA7133-3BD00","Change-over switch 3x 500 A over- lap-WI",5603,"ST",1,"LP",1,"3KA71333BD00"]
["3KA7156-4AA01","INTERRUPTOR SECCIONADOR 4 x 2500 A",5365,"ST",1,"LP",1,"3KA71564AA01"]
["3KA7184-4AA01","Switch disconnector 4x 1600 A W /O HANDLE",6600,"ST",1,"LP",1,"3KA71844AA01"]
["3KC4354-0HA21-0AA3","SENTRON, transfer switching equipment 3KC, remotely operated, RTSE, 3-pole, Iu: 1600 A, Ue AC: 415 V, Ie at AC-33 B at 415 V: 1000 A, Ie at AC-23 A at 690 V: 800 A, screw mounting, motorized operating mechanism, at the right end, long handle, busbar connection",8712,"ST",1,"LP",1,"3KC43540HA210AA3"]
["3KC9000-8TL62","ATC6 expansion module 2DI/2O SSR, Accessory for ATC6300 and ATC6500 pluggable contains 2 digital inputs and 2 solid-state compatible digital outputs 2 NO contacts",268,"ST",1,"LP",1,"3KC90008TL62"]
["3KC9833-3","Accessory for 3KC8 Power supply cable for connection at the bottom 2-pole for 630 A for 3-pole 3KC8 contains 1 unit",219,"ST",1,"LP",1,"3KC98333"]
["3KD2844-2NE10-0","Switch disconnector 80 A, Size 2, 4-pole Lateral operating mechanism left Basic unit without handle Box terminal",90.1,"ST",1,"LP",1,"3KD28442NE100"]
["3KD3630-0NE20-0","Switch disconnector 200 A, Size 2, 3-pole Front operating mechanism center Basic unit without handle flat terminal incl. phase barriers",157,"ST",1,"LP",1,"3KD36300NE200"]
["3KD9001-5","Accessory for 3KD0 size 01/02 door-coupling rotary operating mechanism Complete operating mechanism, gray without tolerance compensation, shaft 6x6, 300mm",20,"ST",1,"LP",1,"3KD90015"]
["3KD9304-5","Accessory for 3KD size 3 3KF size 2, 3KC0 size 3 Cable connection cover short version contains 8 units",38.1,"ST",1,"LP",1,"3KD93045"]
["3KF1308-0LB11","Switch disconnector with fuse 80 A, Size 1, 3-pole for LV HRC fuse Sz. 000 Front operating mechanism left Basic unit without handle Box terminal",203,"ST",1,"LP",1,"3KF13080LB11"]
["3KF5380-4LF11","Switch disconnector with fuse 800 A, Size 5, 3-pole for LV HRC fuse Sz. 2 and 3 Side operating mechanism left Basic unit without handle flat terminal",1377,"ST",1,"LP",1,"3KF53804LF11"]
["3KL7111-3AA00","SECTION FUS-NH 3x 32A SANS COMM",242,"ST",1,"LP",1,"3KL71113AA00"]
["3KL7151-3AE04","Switch disconnector with fuses 3x 630A WI",5094,"ST",1,"LP",1,"3KL71513AE04"]
["3KL7182-4CA01","Switch disconnector with fuses 4x 800A",4325,"ST",1,"LP",1,"3KL71824CA01"]
["3KX3553-3DB01","Terminal cover for 4-pole switch 3KA534 and 3KL534 for M8 thread consists of 8 terminal covers",136.08000000000001,"ST",1,"LP",1,"3KX35533DB01"]
["3KX7133-5AA00","Cache BORNE 3KA71 GR5",49.1,"ST",1,"LP",1,"3KX71335AA00"]
["3KY2232-0A","Spare part for switch 3KE44/45 Arc chute with 3 arc chute inserts",171.32,"ST",1,"LP",1,"3KY22320A"]
["3LD2103-0TK51","SENTRON, Switch disconnector 3LD, main switch, 3-pole, Iu: 25 A, Operating power / at AC-23 A at 400 V: 9.5 kW, front-mounted, rotary operating mechanism, black, 4-hole mounting of the handle",30.6,"ST",1,"LP",1,"3LD21030TK51"]
["3LD2318-1TL13","SENTRON, Switch disconnector 3LD, emergency switching-off switch, 4- pole, Iu: 160 A, operating power / at AC-23 A 400 V: 75 kW, floor mounting with door coupling, knob-operated mechanism, red/yellow, 4-hole mounting of the handle",399,"ST",1,"LP",1,"3LD23181TL13"]
["3LD2585-2GP21","SENTRON switch disconnector 3LD in molded-plastic enclosure , repair and maintenance switch with EMC plate, 3-pole Iu: 63A, AC23A 400V at 50/60Hz: 22kW, used with frequency converter: AC20 400V at 0-550Hz: 18,5kW, 1NO + 1NC 20-150ms leading,β€‹ molded-plastic encapsulation for metric cable gland, knob-operated mechanism, black, lockable in 0- and I-position, incl. cable shield clamps and hose clamps",129,"ST",1,"LP",1,"3LD25852GP21"]
["3LD3050-0TL13","Load disconnector 3LD3, Iu 16 A Main switch 3-pole + N Rated operating capacity at AC-23 A at 400V 7.5kW Front plate mounting Basic switch with Central hole mounting 22.5mm Toggle drive red / yellow 48x48 mm",28.8,"ST",1,"LP",1,"3LD30500TL13"]
["3LD3350-0TK13","Load disconnector 3LD3, Iu 40 A Main switch 3-pole Rated operating capacity at AC-23 A at 400 V 18,5 kW Front plate mounting Basic switch with Central hole mounting 22.5mm Toggle drive red / yellow 48x48 mm",46.3,"ST",1,"LP",1,"3LD33500TK13"]
["3LD5600-0TL11","SENTRON, Molded case switch 3LD5 UL, Main switch, 4-pole, certified according to UL489 UL60947-4-1 and IEC60947-3, UL: 125A, SCCR 65kA at 480VAC, Operating power at 480VAC 3-phase: 75hp, IEC: 125A, Operating power at AC-23A at 400V: 55kW, floor mounting with direct handle, black, incl. terminal covers for the infeed side",266,"ST",1,"LP",1,"3LD56000TL11"]
["3LD9284-3B","rotary operating mechanism, actuating lever Red / yellow, four-hole Front mounting, accessory for main and emergency switching-off switch 3LD2 for 63A - 125A and for molded case switch 3LD UL for 30A",15.9,"ST",1,"LP",1,"3LD92843B"]
["3NA3230","LV HRC fuse element, NH2, In: 100 A, gG, Un AC: 500 V, Un DC: 440 V, Front indicator, live grip lugs",14.6,"ST",1,"LP",3,"3NA3230"]
["3NA3362-6","LV HRC fuse element, NH3, In: 425 A, gG, Un AC: 690 V, Un DC: 440 V, Front indicator, live grip lugs",111,"ST",1,"LP",3,"3NA33626"]
["3NA6817-4","LV HRC fuse element, NH000, In: 40 A, gG, Un AC: 400 V, Combined indicator, insulated Grip lugs",8.32,"ST",1,"LP",3,"3NA68174"]
["3NA7240","LV HRC fuse element, NH2, In: 200 A, gG, Un AC: 500 V, Un DC: 440 V, Combined indicator, live grip lugs",15.5,"ST",1,"LP",3,"3NA7240"]
["3NC1425-5","SITOR cylindrical fuse link, 14x51 mm, 25 A, aR, Un AC: 690 V, Un DC: 600 V, DC according to UL, Striker indicator",26.3,"ST",1,"LP",10,"3NC14255"]
["3NC8434-3C","SITOR fuse link, with slotted blade contacts, NH3, In: 500 A, gR, Un AC: 690 V, Un DC: 440 V, front indicator",258,"ST",1,"LP",3,"3NC84343C"]
["3NE1334-2","SITOR fuse link, with blade contacts, NH2, In: 500 A, gR, Un AC: 690 V, Un DC: 440 V, front indicator",297,"ST",1,"LP",3,"3NE13342"]
["3NE4334-6B","SITOR fuse link, with female thread on both sides, In: 500 A, aR, Un AC: 800 V, Un DC: 440 V, front indicator",228,"ST",1,"LP",3,"3NE43346B"]
["3NH5023","SITOR fuse holder 315 A 690 V 1-pole with bolt terminal with fixing dimension 80 mm",19.5,"ST",1,"LP",3,"3NH5023"]
["3NJ4915-1EA10","Accessory for strips 3NJ41 In-line fuse switch disconnectors Sz. NH00 Current transformers can be integrated 100/1 A, Cl. 0.5",287,"ST",1,"LP",1,"3NJ49151EA10"]
["3NJ6203-1AA00-2DE4","Switch disconnector with fuses In-line design, pluggable NH00 160 A, 3-pole Standard switching capacity S manual operation without auxiliary switch 1 current transformer on 1 ammeter, Bimetal 150/5 A, Cl. 1 1, 2-fold overload",1656.99,"ST",1,"LP",1,"3NJ62031AA002DE4"]
["3NJ6213-4AA00-0AA0","Switch disconnector with fuses In-line design, pluggable NH1 250 A, 3-pole High switching capacity H Motorized operating mechanism without auxiliary switch without current transformer without ammeter",6366.96,"ST",1,"LP",1,"3NJ62134AA000AA0"]
["3NJ6920-3BD21","accessory for Switch disconnector with fuses In-line design, pluggable current transformer 100/5 A, Cl. 1, 2.5 VA",74.599999999999994,"ST",1,"LP",1,"3NJ69203BD21"]
["3NJ6920-3FE00","accessory for Switch disconnector with fuses In-line design, plug-in, NH00 Electronic fuse monitoring and line monitoring EFM 25, for DC networks",590,"ST",1,"LP",1,"3NJ69203FE00"]
["3NP1133-1BB12","SENTRON, Fuse switch disconnector 3NP1, 3-pole, NH00, 160 A, for Busbar system 8US 40 mm, flat terminal, Fuse monitoring: electronic EFM10, Cover level 32/70 mm",329,"ST",1,"LP",1,"3NP11331BB12"]
["3NP1163-1JC13","SENTRON, Fuse switch disconnector 3NP1, 3-pole, NH3, 630 A, for Rittal busbar system 60 mm, flat terminal, Fuse monitoring: electronic EFM20, Cover level 32/70 mm",876,"ST",1,"LP",1,"3NP11631JC13"]
["3NP1933-1EB00","Mounting kit, for conversion to installation on standard mounting rail, for Size NH00 for floor mounting, accessory for fuse switch disconnector 3NP1",10.199999999999999,"ST",1,"LP",1,"3NP19331EB00"]
["3NP1963-1CD00","Cable connection cover with reach-around protection, for size NH3, Accessory for fuse Switch disconnector 3NP1",24.2,"ST",1,"LP",1,"3NP19631CD00"]
["3NP5260-0EB26","SENTRON, Fuse switch disconnector 3NP5, 3-pole, NH1, 250 A, for assembly and installation on mounting plate, with High-speed closing, screw terminal, Fuse monitoring: through 3VU, Auxiliary switch at Switch disconnector: 1 NO+1 NC, Auxiliary switch at the Fuse monitoring: 2 NO",1109,"ST",1,"LP",1,"3NP52600EB26"]
["3NW7903","Auxiliary current switch 1 CO for cylindrical fuse holder Sz. 10 x 38 mm/8 x 32 mm",27.6,"ST",1,"LP",1,"3NW7903"]
["3NX1003","Blanking insert Sz. 00 for LV HRC fuse base Sz. 00",10.9,"ST",1,"LP",3,"3NX1003"]
["3RA1110-0DD15-1AP0","Load feeder fuseless direct-on-line starting, 400 V AC 0.22...0.32 A, 230 V AC 50 Hz Size S00 1 NO (contactor), Screw terminal on 60 mm busbar adapter Type of coordination 2, Iq = 50 kA !!! Phased-out product !!! Successor is SIRIUS 3RA2 Preferred successor type is >>3RA2110-0DD15-1AP0<<",396,"ST",1,"CP",1,"3RA11100DD151AP0"]
["3RA1110-1AD15-1AF0","Load feeder fuseless direct-on-line starting, 400 V AC 1.1...1.6 A, 110 V AC 50 Hz Size S00 1 NO (contactor), Screw terminal on 60 mm busbar adapter Type of coordination 1, Iq = 50 kA !!! Phased-out product !!! Successor is SIRIUS 3RA2",417,"ST",1,"CP",1,"3RA11101AD151AF0"]
["3RA1115-1GA15-1AG6","Load feeder fuseless direct-on-line starting, 400 V AC Size S00 4.5-6.3 A, 100 V AC, 50/60 Hz Screw terminal for installation on standard mounting rail Iq = 50 kA, 1 NO (contactor) 1 NO+1 NC (circuit breaker) !!! Phased-out product !!! Successor is SIRIUS 3RA2",331,"ST",1,"CP",1,"3RA11151GA151AG6"]
["3RA1120-1DA24-0AF0","Load feeder fuseless direct-on-line starting, 400 V AC 2.2...3.2 A, 110 V AC 50 Hz Size S0 Screw terminal for installation on standard mounting rail (also fulfills type of coordination 1) !!! Phased-out product !!! Successor is SIRIUS 3RA2",391,"ST",1,"CP",1,"3RA11201DA240AF0"]
["3RA1120-4BD25-0AB0","Load feeder fuseless direct-on-line starting, 400 V AC 14...19 A, 24 V AC 50 Hz Size S0 Screw terminal on 60 mm busbar adapter Type of coordination 1, Iq = 50 kA !!! Phased-out product !!! Successor is SIRIUS 3RA2",565,"ST",1,"CP",1,"3RA11204BD250AB0"]
["3RA1210-0DC15-0BB4","Load feeder fuseless Reversing operation, 400 V AC 0.22...0.32 A, 24 V DC Size S00 Screw terminal Type of coordination 2, Iq = 50 kA on 40 mm busbar adapter !!! Phased-out product !!! Successor is SIRIUS 3RA2 Preferred successor type is >>3RA2210-0DD15-2BB4<<",655,"ST",1,"CP",1,"3RA12100DC150BB4"]
["3RA1210-1CA15-0BB4","Load feeder fuseless Reversing operation, 400 V AC Size S00 1.8-2.5 A, 24 V DC Screw terminal Type of coordination 1, Iq = 50 kA !!! Phased-out product !!! Successor is SIRIUS 3RA2 Preferred successor type is >>3RA2210-1CA15-2BB4<<",509,"ST",1,"CP",1,"3RA12101CA150BB4"]
["3RA1215-0GL16-0BB4","Load feeder fuseless Reversing operation, 400 V AC 0.45...0.63 A. 24 V DC Size S00 1 NO + 1 NC (circuit breaker) With slide adapter !!! Phased-out product !!! Successor is SIRIUS 3RA2",746,"ST",1,"CP",1,"3RA12150GL160BB4"]
["3RA1220-4BC25-0BB4","Load feeder fuseless Reversing operation, 400 V AC 14...19 A, 24 V DC Size S0 Screw terminal Type of coordination 1, Iq = 50 kA on 40 mm busbar adapter !!! Phased-out product !!! Successor is SIRIUS 3RA2 Preferred successor type is >>3RA2220-4BD26-0BB4<<",1216,"ST",1,"CP",1,"3RA12204BC250BB4"]
["3RA1225-0EL16-4BB4","Load feeder fuseless Reversing operation, 400 V AC Size S00 0.28-0.4 A, 24 V DC 1 NO + 1 NC circuit breaker 2 NC+2 NO (contactor) Screw terminal With slide adapter Circuit breaker size S0 !!! Phased-out product !!! Successor is SIRIUS 3RA2",986,"ST",1,"CP",1,"3RA12250EL164BB4"]
["3RA1316-8XB37-1AF0","Reversing contactor assembly AC-3, 4 kW/400 V,110 V AC, 50/60 Hz 3-pole, Size S00 Screw terminal Electrical and mechanical interlock 2 x 3 NO + 1 NC !!! Phased-out product !!! Successor is SIRIUS 3RA2",293,"ST",1,"CP",1,"3RA13168XB371AF0"]
["3RA1344-8XB30-1AH2","Reversing contactor assembly AC-3, 30 kW/400 V,  3-pole Size S3, Screw terminal 48 V AC/50/60 Hz Electrical and mechanical interlock !!! Phased-out product !!! Successor is SIRIUS 3RA2",945,"ST",1,"CP",1,"3RA13448XB301AH2"]
["3RA1445-8XB20-1AP0","Contactor assembly Star-delta (wye-delta) (pre-assembled) with timing relay on the front AC-3, 75 kW/400 V, 3-pole Size S3, S3, S3 Electrically interlocked Screw terminal 1 NO, 230 V AC, 50 Hz !!! Phased-out product !!! Successor is SIRIUS 3RA2",1890,"ST",1,"CP",1,"3RA14458XB201AP0"]
["3RA2110-0CD15-1AP0","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S00 0.18...0.25 A 230 V AC screw terminal for 60 mm busbar systems (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO (contactor)",129,"ST",1,"CP",1,"3RA21100CD151AP0"]
["3RA2110-1DE15-1AP0","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S00 2.20...3.20 A 230 V AC Spring-type terminal for installation on standard mounting rail (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO (contactor)",106,"ST",1,"CP",1,"3RA21101DE151AP0"]
["3RA2115-1HA15-1EG6","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S00 5.50...8.00 A 100 V, 50 Hz 100...110 V, 60 Hz screw terminal for installation on standard mounting rail (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO (contactor) 1 NO+1 NC (circuit breaker, transverse) Coil with RC element plugged on at the front(contactor)",346,"ST",1,"CP",1,"3RA21151HA151EG6"]
["3RA2120-4BE27-0BB4","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S0 13...20 A 24 V DC Spring-type terminal for installation on standard mounting rail (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO+1 NC (contactor)",243,"ST",1,"CP",1,"3RA21204BE270BB4"]
["3RA2125-4NE27-0FB4","Load feeder fuseless, Direct-on-line starting 400 V AC, Size S0 23...28 A 24 V DC Spring-type terminal for installation on standard mounting rail (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO+1 NC (contactor) with diode combination plugged in at the front",321,"ST",1,"CP",1,"3RA21254NE270FB4"]
["3RA2210-0CH15-2AP0","Load feeder fuseless, Reversing duty 400 V AC, Size S00 0.18...0.25 A 230 V AC Spring-type terminal for 60 mm busbar systems (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NC (contactor)",199,"ST",1,"CP",1,"3RA22100CH152AP0"]
["3RA2210-1GD15-2BB4","Load feeder fuseless, Reversing duty 400 V AC, Size S00 4.50...6.30 A 24 V DC screw terminal for 60 mm busbar systems Type of coordination 1, Iq = 150 kA 1 NC (contactor)",222,"ST",1,"CP",1,"3RA22101GD152BB4"]
["3RA2220-4EF27-0BB4","Load feeder fuseless, Reversing duty 400 V AC, Size S0 27.0...32.0 A 24 V DC Spring-type terminal for installation on standard mounting rail with standard mounting rail adapter (also fulfills type of coordination 1) Type of coordination 2, Iq = 150 kA 1 NO+1 NC (contactor)",501,"ST",1,"CP",1,"3RA22204EF270BB4"]
["3RA2316-8XB34-1CF0","Reversing contactor assembly AC-3,4 kW/400 V,AC110V,50/60 Hz 3-pole, Size S00 screw terminal electrical and mechanical interlock with 2x front-side auxiliary switch Varistor plugged on",155,"ST",1,"CP",1,"3RA23168XB341CF0"]
["3RA2324-8XB30-2AG2","Reversing contactor assembly AC-3, 5.5 kW/400 V,AC110V,50/60Hz 3-pole, Size S0 Spring-type terminal electrical and mechanical interlock",128,"ST",1,"CP",1,"3RA23248XB302AG2"]
["3RA2345-8XB30-1AG2","Reversing contactor assembly, AC-3, 37 kW 400 V, 110 V AC/50/60 Hz 3-pole, Size S3 screw terminal electrical and mechanical interlock 2 NO integrated",557,"ST",1,"CP",1,"3RA23458XB301AG2"]
["3RA2446-8XF32-1AC2","Contactor assembly for star-delta (wye-delta) start AC-3, 90 kW/400 V 24 V AC/50/60 Hz Size S3, screw terminal electrical and mechanical interlock 3 NO+3 NC",1127,"ST",1,"CP",1,"3RA24468XF321AC2"]
["3RA2913-2AA1","Wiring kit for screw terminal Electrical and mechanical Including mechanical interlocking for reversing starter Size S00",29.8,"ST",1,"CP",1,"3RA29132AA1"]
["3RA6120-2BE34","SIRIUS Compact load feeder DOL starter 690 V 42...70 V AC/DC 50...60 Hz 0.32...1.25 A IP20 Connection main circuit: Spring-type terminal Connection auxiliary circuit: plug-in, without terminals",803,"ST",1,"CP",1,"3RA61202BE34"]
["3RA6250-1EB33","SIRIUS Compact load feeder Reversing starter 400 V 24 V AC/DC 50...60 Hz 8...32 A IP20 Connection main circuit: plug-in, without terminals Connection control circuit: screw terminal",1095,"ST",1,"CP",1,"3RA62501EB33"]
["3RA6250-2EE34","SIRIUS Compact load feeder Reversing starter 400 V 42...70 V AC/DC 50...60 Hz 8...32 A IP20 Connection main circuit: Spring-type terminal Connection control circuit: plug-in, without terminals",2103,"ST",1,"CP",1,"3RA62502EE34"]
["3RB2036-2QW1","Overload relay 6...25 A For motor protection Size S2, Class 20 Stand-alone installation Main circuit: straight-through transformer Auxiliary circuit: Screw terminal Manual-Automatic-Reset !!! Phased-out product !!! Successor is SIRIUS 3RB3 Preferred successor type is >>3RB3026-2QB0<<",203,"ST",1,"CP",1,"3RB20362QW1"]
["3RB3036-1WB0","Overload relay 20...80 A Electronic For motor protection Size S2, Class 10E Contactor mounting Main circuit: Screw Auxiliary circuit: Screw Manual-Automatic-Reset",196,"ST",1,"CP",1,"3RB30361WB0"]
["3RB3123-4VE0","Overload relay 10...40 A Electronic For motor protection Size S0, Class 5...30 Contactor mounting Main circuit: Spring-type terminal Auxiliary circuit: Spring-type terminal Manual-Automatic-Reset Internal ground fault detection",180,"ST",1,"CP",1,"3RB31234VE0"]
["3RF2120-1BA44-1KS0","Semiconductor relay, 1-phase 3RF2 Width 22.5 mm, 20 A 48-460 V / 5 V DC screw terminal Instantaneous switching",96.8,"ST",1,"CP",1,"3RF21201BA441KS0"]
["3RF2320-2AA24","Solid-state contactor 1-phase 3RF2 AC 51 / 20 A / 40 Β°C 48-460 V / 110-230 V AC Spring-type terminal",78.099999999999994,"ST",1,"CP",1,"3RF23202AA24"]
["3RF2340-3AA22","Solid-state contactor 1-phase 3RF2 AC 51 / 40 A / 40 Β°C 24-230 V / 110-230 V AC Ring cable connection",86,"ST",1,"CP",1,"3RF23403AA22"]
["3RF2420-2AB55","Solid-state contactor 3-phase 3RF2 AC 51 / 20 A / 40 Β°C 48-600 V / 230 V AC 2-phase controlled Spring-type terminal Blocking voltage 1200 V",176,"ST",1,"CP",1,"3RF24202AB55"]
["3RG9101-0BH16","AS-Interface user module Kit upper part for EAO-ESA-LUMITAS",9.4,"ST",1,"CP",1,"3RG91010BH16"]
["3RH1122-2KG40-0LA4","Contactor with VDR 2 NO + 2 NC Railway 87...156 V, spring-loaded connection technology, !!! Phased-out product !!! Successor is SIRIUS 3RH2 Preferred successor type is >>3RH2122-2KG40-0LA4<<",181,"ST",1,"CP",1,"3RH11222KG400LA4"]
["3RH1140-1AF00-0AA6","Contactor relay, 2 NO + 2 NC, 110 V AC, 50 / 60 Hz, screw terminal, Size S00 Reinforced standard mounting rail installation !!! Phased-out product !!! Successor is SIRIUS 3RH2",207,"ST",1,"CP",1,"3RH11401AF000AA6"]
["3RH1344-1AP00-0KA0","Contactor relay, 230 V AC, 50 / 60 Hz, screw terminal, Size S00 2 NO + 2 NC basic unit / EN !!! Phased-out product !!! Successor is SIRIUS 3RH2 Preferred successor type is >>3RH2344-1AP00-0KA0<<",125,"ST",1,"CP",1,"3RH13441AP000KA0"]
["3RH1921-1HK22","ATTACHABLE CONTACT BLOCK, 4POLE 2NO+1NC A. 1NC(AFTER/2ND POLE) SCREW CONNECTION FOR MOTOR CONTACTORS,",26.8,"ST",1,"CP",1,"3RH19211HK22"]
["3RH2122-1BA40-0AA6","Contactor relay, 2 NO + 2 NC, 12 V DC, Size S00, screw terminal reinforced standard mounting rail installation",81.099999999999994,"ST",1,"CP",1,"3RH21221BA400AA6"]
["3RH2122-2AP00-1AA0","Contactor relay, 2 NO + 2 NC, 230 V AC, 50 / 60 Hz, Size S00, Spring-type terminal upright mounting position",35.1,"ST",1,"CP",1,"3RH21222AP001AA0"]
["3RH2131-2VB40","Coupling contactor relay, 3 NO + 1 NC, 24 V DC, 0.85 ... 1.85* US, with integrated diode, Size S00, Spring-type terminal",43,"ST",1,"CP",1,"3RH21312VB40"]
["3RH2140-2BB40","Contactor relay, 4 NO, 24 V DC, Size S00, Spring-type terminal",37.300000000000004,"ST",1,"CP",1,"3RH21402BB40"]
["3RH2344-1CH00","Contactor relay with auxiliary switch 48 V AC, 50 / 60 Hz Size S00, screw terminal, 4 NC basic unit / EN Varistor plugged on",64.3,"ST",1,"CP",1,"3RH23441CH00"]
["3RH2911-1DA11","Auxiliary switch lateral, 1 NO + 1 NC Current path 1 NC, 1 NO for 3RH and 3RT screw terminal R: 21/22, 33/34 L: 41/42, 53/54",14.5,"ST",1,"CP",1,"3RH29111DA11"]
["3RH2921-1DA20","Auxiliary switch lateral, 2 NO Current path 1 NO, 1 NO for 3RH and 3RT screw terminal R: 33/34, 43/44 L: 53/54, 63/64",14.5,"ST",1,"CP",1,"3RH29211DA20"]
["3RK1301-0AB10-1AB4","RS1E-X for ET200S High Feature reversing starter Setting range 0.3...3 A Mechanical switching Electronic protection AC-3, up to 1.1 kW / 400 V expandable for Brake control module 2DI module 2DI module Circuit breaker signaling parameterizable DPV 1-capable PROFIENERGY-capable to PN",880,"ST",1,"CP",1,"3RK13010AB101AB4"]
["3RK1303-6DS71-1AA3","ECOFAST reversing starter PROFIBUS DP Electronic switching Electronic/thermal Overload protection AC-3, up to 5.5 kW / 400 V 2.40 A to 12.00 A Break contact AC 400 V/0.75 A for internally supplied brakes Digital input DI 2 x 24 V DC Metal enclosure (lower part)",11829,"ST",1,"CP",1,"3RK13036DS711AA3"]
["3RK1308-0DA00-0CP0","Failsafe reversing starter High Feature; Electronic switching; Electronic overload protection up to 0.09 kW / 400 V; Adjustment range 0.1 .. 0.4 A; PROFIenergy; Option: 3DI/LC module",647,"ST",1,"CP",1,"3RK13080DA000CP0"]
["3RK1400-1BQ00-0AA3","AS-i compact module K60 digital 2 DI/2 DQ, IP67 2 x 1 input, max. 200 mA 2 x 1 output, 2 A, 24 V DC 2 x M12 standard socket Y assignment Mounting plate 3RK1901-0CA00 must be ordered separately",261,"ST",1,"CP",1,"3RK14001BQ000AA3"]
["3RK1408-8KG00-0AA2","AS-i ground fault module IP20 S22.5, ground fault monitoring 1 input, remote reset 2 x signaling output, Relay DC-12 1 A / DC-13 500 mA (24 V) Spring-type terminal Overall width 22.5 mm No AS-i address required Only AS-Interface monitoring",203,"ST",1,"CP",1,"3RK14088KG000AA2"]
["3RK1901-2NR10","AS-Interface M12 branch U_ASI without Uaux, with M12 socket IP67/68/69K, max. 4 A",33.4,"ST",1,"CP",1,"3RK19012NR10"]
["3RK1903-0CH20","2 DI 24 V DC LC COM Control module for ET200S High Feature Starter for ET 200S Failsafe Starter for local input functions or for manual operation with COM interface for PC cable 6ED1057-1 AA00-0BA0",250,"ST",1,"CP",1,"3RK19030CH20"]
["3RK1911-0CG30","ECOFAST motor connection cables 7 x 1.5 mm2 pre-assembled single-sided Han 10E Any length, >3 m to <5 m Length specification when ordering Grid at least 10 cm",417,"ST",1,"CP",1,"3RK19110CG30"]
["3RK1911-4AA16","ECOFAST Selective block for selective switching-off Maintenance switch function rated current 16 A AS-Interface connection",1769,"ST",1,"CP",1,"3RK19114AA16"]
["3RK4320-3EQ54-1BA3","SIRIUS MCU motor starter Enclosure degree of protection IP54 metal Communication AS-Interface electromechanically switching Short-circuit protection with circuit breaker Reversing starter Brake 400 V AC (internal) Performance class 1.60 A Motor circuit breaker with bi-metal thermal Rotary operating mechanism gray/black Connection power M screw connection Standard product",4452,"ST",1,"CP",1,"3RK43203EQ541BA3"]
["3RK4324-3CR51-0BC0","SIRIUS MCU motor starter Enclosure degree of protection IP54 plastic Communication AS-Interface electromechanically switching Short-circuit protection with circuit breaker DOL starter Brake without Performance class 1 A Motor circuit breaker with bi-metal thermal without manual operation Connection power M screw connection Special variant new design A/B slave AS-i SPEC V2.1 Sensor-actuator 1x AS-i 3xDI/DO Supply sensor U-AUX",1243,"ST",1,"CP",1,"3RK43243CR510BC0"]
["3RK4324-3PR54-1BC0","SIRIUS MCU motor starter Enclosure degree of protection IP54 plastic Communication AS-Interface electromechanically switching Short-circuit protection with circuit breaker Reversing starter Brake without Performance class 12 A Motor circuit breaker with bi-metal thermal with manual operation Connection power M screw connection Special variant new design A/B slave AS-i SPEC V2.1 Sensor-actuator 1x AS-i 1xDI/DO Supply sensor U-AUX",1348,"ST",1,"CP",1,"3RK43243PR541BC0"]
["3RM1102-3AA04","Fail-safe direct starter, 3RM1, 500 V, 0.09 - 0.75 kW, 0.4 - 2 A, 24 V DC, screw/spring-type terminals",196,"ST",1,"CP",1,"3RM11023AA04"]
["3RN1011-2BG00","!!! Phased-out product !!! The preferred successor is 3RN2011-2BW30 Thermistor motor protection Standard evaluation unit Manual/remote 2 W, 110 V AC",181,"ST",1,"CP",1,"3RN10112BG00"]
["3RP1555-2AQ30","Timing relay, Multifunction Phased-out product !!! For further information, please contact our sales department Spring-type terminal 1 change-over contact clock generator 0.5 s...100 h 24 V AC/DC, 100-127 V AC with LED, at 50/60 Hz AC",325,"ST",1,"CP",1,"3RP15552AQ30"]
["3RP2505-2CW30","Timing relay, Multifunction 1 NO semiconductor 13 functions 7 time ranges (0.05 s...100 h) 12-240 V AC/DC at 50/60 Hz AC with LED, Spring-type terminal (push-in)",113,"ST",1,"CP",1,"3RP25052CW30"]
["3RQ3070-1SG30","Input coupler Optocoupler 1 NO contact, Transistor Input 110-230 V AC/DC Output max. 30 V DC, 0.5 A short circuit-proof Overall width 6.2 mm screw terminal Thermal current 0.5 A",72.899999999999991,"ST",1,"CP",1,"3RQ30701SG30"]
["3RS1121-1DD40","Temperature monitoring relay Thermocouple type K, overshoot 2 threshold values, Width 22.5 mm 500 Β°C to 1000 Β°C 24 V AC/DC 1 NO + 1 CO, Load and quiescent current screw terminal",282,"ST",1,"CP",1,"3RS11211DD40"]
["3RS1800-2BW00","!!! Phased-out product !!! The preferred successor is 3RQ2000-2BW00. Coupling relays in industrial enclosure 2 change-over contacts Wide voltage range 24 V to 240 V AC/DC Spring-type terminal",80.5,"ST",1,"CP",1,"3RS18002BW00"]
["3RS7006-1FW00","Separation amplifier 24-240 V AC/DC, 3-way separation input: 0-60 mV, 0-100 mV 0-300 mV, 0-500 mV, 0-1 V 0-20 V, 2-10 V, 0-5 mA, 0-10 mA  2-10 V, 0-5 mA, 0-10 mA 0-20mA, 4-20 mA, +-5 mA, +-20 mA output: 0 - 10 V, 0/4 - 20 mA screw terminal",336,"ST",1,"CP",1,"3RS70061FW00"]
["3RT1034-3AG18-0PA3","Power contactor, AC-3 32 A, 15 kW / 400 V 3 NO + 2 NC, 3-pole, Size S3, Main circuit: Screw terminal Auxiliary circuit: Spring-type terminal Aux. switch 3 NO + 3 NC, lateral !!! Phased-out product !!! Successor is SIRIUS 3RT2",327,"ST",1,"CP",1,"3RT10343AG180PA3"]
["3RT1035-1AL20-1AA0","Power contactor, AC-3 40 A, 18.5 kW / 400 V 230 V AC, 50 / 60 Hz, 3-pole, Size S2, Screw terminal Upright mounting position !!! Phased-out product !!! Successor is SIRIUS 3RT2",241,"ST",1,"CP",1,"3RT10351AL201AA0"]
["3RT1035-3AG14","Power contactor, AC-3 40 A, 18.5 kW / 400 V 110 V AC, 60 Hz, 3-pole, Size S2, 2 NO + 2 NC, Main circuit: Screw terminal Auxiliary circuit: Spring-type terminal !!! Phased-out product !!! Successor is SIRIUS 3RT2",256,"ST",1,"CP",1,"3RT10353AG14"]
["3RT1036-1AH20-1AA0","Power contactor, AC-3 50 A, 22 kW / 400 V 48 V AC, 50 / 60 Hz, 3-pole, Size S2, Screw terminal Upright mounting position !!! Phased-out product !!! Successor is SIRIUS 3RT2",317,"ST",1,"CP",1,"3RT10361AH201AA0"]
["3RT1044-1AP64","Power contactor, AC-3 65 A, 30 kW / 400 V 220 V AC, 50 Hz / 240 V, 60 Hz, 2 NO + 2 NC, 3-pole, Size S3, Screw terminal !!! Phased-out product !!! Successor is SIRIUS 3RT2 Preferred successor type is >>3RT2037-1AP64<<",418,"ST",1,"CP",1,"3RT10441AP64"]
["3RT1044-1BD44","Power contactor, AC-3 65 A, 30 kW / 400 V 42 V DC, 2 NO + 2 NC, 3-pole, Size S3, Screw terminal !!! Phased-out product !!! Successor is SIRIUS 3RT2",636,"ST",1,"CP",1,"3RT10441BD44"]
["3RT1045-1AP08-0MA0","Power contactor, AC-3 80 A, 37 kW / 400 V 230 V AC, 50 Hz, 2 NO + 2 NC 3-pole, Size S3 Screw terminal Operating range 0.9-1.1 Us Special-purpose device !!! Phased-out product !!! Successor is SIRIUS 3RT2",498,"ST",1,"CP",1,"3RT10451AP080MA0"]
["3RT1045-3XB40-0LA2","Power contactor, AC-3 80 A, 37 kW / 400 V 24 V DC, 0.7-1.25* Us 3-pole, Size S3 Spring-type terminal With electronic control unit Integrated varistor !!! Phased-out product !!! Successor is SIRIUS 3RT2 Preferred successor type is >>3RT2038-3XB40-0LA2<<",916,"ST",1,"CP",1,"3RT10453XB400LA2"]
["3RT1054-2AD36","Power contactor, AC-3 115 A, 55 kW / 400 V AC (50-60 Hz) / DC operation 42-48 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, Size S6 Busbar connections Drive: conventional Spring-type terminal",395,"ST",1,"CP",1,"3RT10542AD36"]
["3RT1055-2AU36","Power contactor, AC-3 150 A, 75 kW / 400 V AC (50-60 Hz) / DC operation 240-277 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, Size S6 Busbar connections Drive: conventional Spring-type terminal",447,"ST",1,"CP",1,"3RT10552AU36"]
["3RT1056-2NB36","Power contactor, AC-3 185 A, 90 kW / 400 V AC (50-60 Hz) / DC operation 21-27 UC, 3 V Auxiliary contacts 2 NO + 2 NC 3-pole, Size S6 Busbar connections Drive: electronic with PLC interface 24 V DC Spring-type terminal",620,"ST",1,"CP",1,"3RT10562NB36"]
["3RT1075-2AU36","Power contactor, AC-3 400 A, 200 kW / 400 V AC (50-60 Hz) / DC operation 240-277 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, Size S12 Busbar connections Drive: conventional Spring-type terminal",1360,"ST",1,"CP",1,"3RT10752AU36"]
["3RT1076-2AD36","Power contactor, AC-3 500 A, 250 kW / 400 V AC (50-60 Hz) / DC 42-48 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, size S12 Busbar connections Operating mechanism: conventional Spring-type terminals",1669,"ST",1,"CP",1,"3RT10762AD36"]
["3RT1276-6AB36","Vacuum contactor, AC-3 500 A, 250 kW / 400 V AC (50-60 Hz) / DC operation 23-26 V UC Auxiliary contacts 2 NO + 2 NC 3-pole, Size S12 Busbar connections Drive: conventional",2784,"ST",1,"CP",1,"3RT12766AB36"]
["3RT1346-1AV00","Contactor, AC-1, 140 A, 400 V AC, 50 Hz, 4-pole, Size S3, Screw terminal !!! Phased-out product !!! Successor is SIRIUS 3RT2 Preferred successor type is >>3RT2346-1AV00<<",706,"ST",1,"CP",1,"3RT13461AV00"]
["3RT1466-6SP36","Contactor, AC-1, 400 A/690 V/40 Β°C, S10, 3-pole, 200-277 V AC/DC, F-PLC-IN with varistor, 2 NO+2 NC, Connection rail/ screw terminal",1203,"ST",1,"CP",1,"3RT14666SP36"]
["3RT1916-4KA6","Soldering pin adapter for contactors with mounted 4-pole auxiliary switch block for 3RT101.1. with 3.8 mm long soldering pins consists of 4 adapters for 1 contactor !!! Phased-out product !!! Successor is SIRIUS 3RT2",11.5,"ST",1,"CP",4,"3RT19164KA6"]
["3RT1934-5AP02","Magnet coil for contactors SIRIUS, Size S2, spring-loaded connection technology 230 V AC, 50 Hz !!! Phased-out product !!! Successor is SIRIUS 3RT2",35.300000000000004,"ST",1,"CP",1,"3RT19345AP02"]
["3RT1944-6E","Replacement contact pieces for contactor Size S3, main contacts 4 NO, AC-1, 110 A, consists of 4 movable and 8 fixed contacts with mounting parts !!! Phased-out product !!! Successor is SIRIUS 3RT2",228,"ST",1,"CP",1,"3RT19446E"]
["3RT1955-5AF32","Changeover operating mechanism for contactors 3RT105, 3RT145 AC (50...60 Hz) / DC operation, 110 ... 127 V Operating mechanism: Standard,economy circuit Spring-type terminal",118,"ST",1,"CP",1,"3RT19555AF32"]
["3RT1965-5NF31","Changeover operating mechanism for contactors 3RT106, 3RT146 AC (50...60 Hz) / DC operation, 96 ... 127 V Operating mechanism: electronic with PLC input 24 V DC Screw terminal",255,"ST",1,"CP",1,"3RT19655NF31"]
["3RT2015-1BB42-0CC0","Power contactor, AC-3 7 A, 3 kW / 400 V 1 NC, 24 V DC communication-capable, 3-pole, Size S00, screw terminal",37,"ST",1,"CP",1,"3RT20151BB420CC0"]
["3RT2015-1MB42-0KT0","power contactor, AC-3 7 A, 3 kW / 400 V 1 NC, 24 V DC 0.85-1.85* US, 3-pole, size S00, screw terminal not expandable with auxiliary switch",33.300000000000004,"ST",1,"CP",1,"3RT20151MB420KT0"]
["3RT2016-1AF01-1AA0","Power contactor, AC-3 9 A, 4 kW / 400 V 1 NO, 110 V AC, 50/60 Hz 3-pole, Size S00 screw terminal upright mounting position",32.5,"ST",1,"CP",1,"3RT20161AF011AA0"]
["3RT2016-1FB41","Power contactor, AC-3 9 A, 4 kW / 400 V 1 NO, 24 V DC with diode integrated, 3-pole, Size S00, screw terminal",39.800000000000004,"ST",1,"CP",1,"3RT20161FB41"]
["3RT2017-1BB44-3MA0","Power contactor, AC-3 12 A, 5.5 kW / 400 V 2 NO + 2 NC, 24 V DC 3-pole, Size S00 Screw terminal Captive auxiliary switch",55.4,"ST",1,"CP",1,"3RT20171BB443MA0"]
["3RT2017-2AP01","power contactor, AC-3 12 A, 5.5 kW / 400 V 1 NO, 230 V AC, 50 / 60 Hz 3-pole, Size S00 Spring-type terminal",33.700000000000003,"ST",1,"CP",1,"3RT20172AP01"]
["3RT2017-2XB41-0LA2","Traction contactor, AC-3 12 A, 5.5 kW / 400 V 1 NO, 24-34 V DC, 0.7-1.25*US with integrated varistor Size S00, Spring-type terminal suitable for PLC outputs",60.300000000000004,"ST",1,"CP",1,"3RT20172XB410LA2"]
["3RT2018-2BA41","Power contactor, AC-3 16 A, 7.5 kW / 400 V 1 NO, 12 V DC 3-pole, Size S00 Spring-type terminals",75.399999999999991,"ST",1,"CP",1,"3RT20182BA41"]
["3RT2023-2AG20","power contactor, AC-3 9 A, 4 kW / 400 V 1 NO + 1 NC, 110 V AC 50 / 60 Hz, 3-pole Size S0, Spring-type terminal",32.6,"ST",1,"CP",1,"3RT20232AG20"]
["3RT2024-1BG40","power contactor, AC-3 12 A, 5.5 kW / 400 V 1 NO + 1 NC, 125 V DC 3-pole, Size S0 screw terminal",74.399999999999991,"ST",1,"CP",1,"3RT20241BG40"]
["3RT2024-2BM40","power contactor, AC-3 12 A, 5.5 kW / 400 V 1 NO + 1 NC, 220 V DC 3-pole, Size S0 Spring-type terminal",70.899999999999991,"ST",1,"CP",1,"3RT20242BM40"]
["3RT2025-2BF44","power contactor, AC-3 17 A, 7.5 kW / 400 V 2 NO + 2 NC, 110 V DC, 3-pole, Size S0 Spring-type terminal Removable auxiliary switch",102,"ST",1,"CP",1,"3RT20252BF44"]
["3RT2026-2AV00","power contactor, AC-3 25 A, 11 kW / 400 V 1 NO + 1 NC, 400 V AC, 50 Hz 3-pole, Size S0 Spring-type terminal",70.8,"ST",1,"CP",1,"3RT20262AV00"]
["3RT2027-1AC24","Power contactor, AC-3 32 A, 15 kW / 400 V 2 NO + 2 NC, 24 V AC 50/60 Hz, 3-pole Size S0, screw terminals Removable auxiliary switch",108,"ST",1,"CP",1,"3RT20271AC24"]
["3RT2027-2AG24","Contactor, AC-3, 15 kW / 400 V, 2 NO + 2 NC, 110 V AC, 50 / 60 Hz, 3-pole, Size S0, Spring-type terminal Removable auxiliary switch",108,"ST",1,"CP",1,"3RT20272AG24"]
["3RT2028-2FB40","Power contactor, AC-3 38 A, 18.5 kW / 400 V 1 NO + 1 NC, 24 V DC with plugged-in diode combination, 3-pole size S0 Spring-type terminals",170,"ST",1,"CP",1,"3RT20282FB40"]
["3RT2035-1SF30","contactor, AC-3, 40 A/400 V/60 Β°C S2, 3-pole, 83-150 V AC/DC, F-PLC-IN, with varistor, 1 NC, screw terminal",255,"ST",1,"CP",1,"3RT20351SF30"]
["3RT2036-1SF30","contactor, AC-3, 50 A/400 V/60 Β°C S2, 3-pole, 83-150 V AC/DC, F-PLC-IN, with varistor, 1 NC, screw terminal",348,"ST",1,"CP",1,"3RT20361SF30"]
["3RT2037-3AK60","Contactor, AC-3, 30 kW / 400 V, 1 NO + 1 NC, 110 V AC, 50 Hz / 120 V, 60 Hz, 3-pole, Size S2, Spring-type terminal",200,"ST",1,"CP",1,"3RT20373AK60"]
["3RT2038-1XB40-0LA2","Traction contactor, AC-3 80 A, 37 kW / 400 V 1 NO + 1 NC 24 V DC, 0.7-1.25* Us, with varistor 3-pole, Size S2, screw terminals",502,"ST",1,"CP",1,"3RT20381XB400LA2"]
["3RT2045-1CP04-3MA0","power contactor, AC-3 80 A, 37 kW / 400 V 2 NO + 2 NC, 230 V AC/50 Hz 3-pole, 3 NO, Size S3 screw terminal Inserted varistor Captive auxiliary switch",265,"ST",1,"CP",1,"3RT20451CP043MA0"]
["3RT2046-1AQ20","power contactor, AC-3 95 A, 45 kW / 400 V 2 NO + 1 NC, 500 V AC, 50/60 Hz 3-pole, 3 NO, Size S3 screw terminal",307,"ST",1,"CP",1,"3RT20461AQ20"]
["3RT2317-1AP00","Contactor, AC-1, 22 A/400 V/40 Β°C, S00, 4-pole, 230 V AC, 50/60 Hz, screw terminal",39.4,"ST",1,"CP",1,"3RT23171AP00"]
["3RT2325-2AP60","Contactor, AC-1, 35 A/400 V/40 Β°C, S0, 4-pole, 220 V AC/50 Hz, 240 V/60 Hz, 1 NO+1 NC, Spring-type terminal",63,"ST",1,"CP",1,"3RT23252AP60"]
["3RT2336-1AC20","Contactor, AC-1, 60 A/400 V/40 Β°C, S2, 4-pole, 24 V AC, 50/60 Hz, 1 NO+1 NC, screw terminal",195,"ST",1,"CP",1,"3RT23361AC20"]
["3RT2448-1AL20","Contactor, AC-1, 160 A/690 V/40 Β°C, S3, 3-pole, 230 V AC, 50/60 Hz, 1 NO+1 NC, box terminal/screw terminal",318,"ST",1,"CP",1,"3RT24481AL20"]
["3RT2544-1AF00","Contactor, AC-3, 30 kW/400 V 110 V AC/50 Hz 4-pole, 2 NO+2 NC, Size S3 Screw terminal 1 NO+1 NC integrated",217,"ST",1,"CP",1,"3RT25441AF00"]
["3RT2637-1NP35","Capacitor contactor, AC-6b 75 kVAr, / 400 V 2 NC, 50-60 Hz AC / 175-280 V DC 3-pole, Size S2 screw terminal",627,"ST",1,"CP",1,"3RT26371NP35"]
["3RT2926-2PR11","pneumatic time relay block OFF delay 1 ... 60 s 1 NO + 1 NC, for motor contactors size S0 !!! phased-out product !!! successor 3RT2927-2PR11",123,"ST",1,"CP",1,"3RT29262PR11"]
["3RT2936-1BF00","Surge suppressor, varistor, 400 ... 600 V AC, for contactors Size S2, S3",16.700000000000003,"ST",1,"CP",1,"3RT29361BF00"]
["3RU1136-1HD0","Overload relay 5.5...8 A For motor protection Size S2, Class 10 Contactor mounting Main circuit: Screw terminal Auxiliary circuit: Spring-type terminal Manual-Automatic-Reset !!! Phased-out product !!! Successor is SIRIUS 3RU2 Preferred successor type is >>3RU2126-1HC0<<",117,"ST",1,"CP",1,"3RU11361HD0"]
["3RU2116-0FB1","Overload relay 0.35...0.50 A Thermal For motor protection Size S00, Class 10 Stand-alone installation Main circuit: Screw Auxiliary circuit: Screw Manual-Automatic-Reset",58.7,"ST",1,"CP",1,"3RU21160FB1"]
["3RU2136-1HD0","Overload relay 5.5...8 A Thermal For motor protection Size S2 Class 10 Contactor mounting Main circuit: screw terminal Auxiliary circuit: spring-type terminal Manual-Automatic-Reset",61.7,"ST",1,"CP",1,"3RU21361HD0"]
["3RV1011-0BA20","Circuit breaker size S00 for motor protection CLASS 10 A-release 0.14...0.2 A Short-circuit release 2.6 A Spring-type terminal Standard switching capacity !!! Phased-out product !!! Successor is SIRIUS 3RV2 Preferred successor type is >>3RV2011-0BA20<<",134,"ST",1,"CP",1,"3RV10110BA20"]
["3RV1011-0KA15","Circuit breaker size S00 for motor protection, CLASS 10 A-release 0.9...1.25 A N-release 16 A 1 NO+1 NC transverse Screw terminal Standard switching capacity",71.699999999999989,"ST",1,"CP",1,"3RV10110KA15"]
["3RV1031-4FA10","Circuit breaker size S2 for motor protection, Class 10 A-release 28...40 A Short-circuit release 520 A Screw terminal Standard switching capacity !!! Phased-out product !!! Successor is SIRIUS 3RV2 Preferred successor type is >>3RV2031-4UA10<<",337,"ST",1,"CP",1,"3RV10314FA10"]
["3RV1342-4MC10-0FB0","Circuit breaker size S3 For starter combination Rated current 100 A Short-circuit release 1235 A Screw terminal Increased switching capacity ABB",656,"ST",1,"CP",1,"3RV13424MC100FB0"]
["3RV1821-0KD10","CIRCUIT-BREAKER, SIZE S0, FOR THE TRANSFORMER PROTECTION, WITH APPROBATION CIRC.-BREAKER UL 489, CSA C22.2 NO.5-02, A-TRIGGER 1.25 A, N-TRIGGER 26 A, SCREW CONNECTION, STANDARD BREAKING CAPACITY",374,"ST",1,"CP",1,"3RV18210KD10"]
["3RV1902-1AV00-0FQ0","Undervoltage release 400 V AC/50 Hz, 440 V AC/60 Hz for circuit breaker Size S00...S3 ABB LOVATO",61.9,"ST",1,"CP",1,"3RV19021AV000FQ0"]
["3RV1975-2DA0","Extended cable connection on the front, 6 units for size 3RV1. 73-7J",291,"ST",1,"CP",1,"3RV19752DA0"]
["3RV2011-1BA10","Circuit breaker size S00 for motor protection, CLASS 10 A-release 1.4...2 A N-release 26 A screw terminal Standard switching capacity",53.2,"ST",1,"CP",1,"3RV20111BA10"]
["3RV2011-1HA40","Circuit breaker size S00 for motor protection, CLASS 10 A-release 5.5...8 A N-release 104 A ring cable lug connection Standard switching capacity",58.800000000000004,"ST",1,"CP",1,"3RV20111HA40"]
["3RV2021-1HA20","Circuit breaker size S0 for motor protection, CLASS 10 A-release 5.5...8 A N-release 104 A Spring-type terminal Standard switching capacity",57.5,"ST",1,"CP",1,"3RV20211HA20"]
["3RV2042-4FA10","Circuit breaker size S3 for motor protection, CLASS 10 A-release 28...40 A N-release 520 A screw terminal Increased switching capacity 100 kA",310,"ST",1,"CP",1,"3RV20424FA10"]
["3RV2111-1FA10","Circuit breaker size S00 for motor protection, CLASS 10 with overload relay function A-release 3.5...5 A N release 65 A screw terminal Standard switching capacity",86,"ST",1,"CP",1,"3RV21111FA10"]
["3RV2321-4DC10","Circuit breaker size S0 for starter combination Rated current 25 A N-release 325 A Screw terminal Standard switching capacity",59.1,"ST",1,"CP",1,"3RV23214DC10"]
["3RV2411-1AA15","Circuit breaker size S00 for transformer protection A-release 1.1...1.6 A N-release 33 A screw terminal Standard switching capacity with transverse auxiliary switches 1 NO+1 NC",74.2,"ST",1,"CP",1,"3RV24111AA15"]
["3RV2811-1JD10","Circuit breaker size S00 for transformer protection with approval circuit breaker UL 489, CSA C22.2 No.5-02 A-release 10 A N-release 208 A screw terminal Standard switching capacity",152,"ST",1,"CP",1,"3RV28111JD10"]
["3RV2926-3C","door-coupling rotary operating mechanism for harsh conditions for circuit breaker size S00/S0 handle EMERGENCY OFF",102,"ST",1,"CP",1,"3RV29263C"]
["3RW3014-2BB14","SIRIUS soft starter S00 6.5 A, 3 kW/400 V, 40 Β°C 200-480 V AC, 110-230 V AC/DC spring-type terminals",190,"ST",1,"CP",1,"3RW30142BB14"]
["3RW4056-6BB34","SIRIUS soft starter S6 145 A, 100 hp/460 V, 50 Β°C 200-460 V AC, 115 V AC Screw terminals !!! Phased-out product !!! Successor is SIRIUS 3RW5, Preferred successor type is >>3RW5056-6AB14<<",2103,"ST",1,"CP",1,"3RW40566BB34"]
["3RW4422-3BC35","SIRIUS soft starter Values at 575 V, 50 Β°C standard: 26 A, 20 hp Inside-delta: 45 A, 40 hp 400-600 V AC, 115 V AC spring-type terminals !!! Phased-out product !!! Successor is SIRIUS 3RW5, Preferred successor type is >>3RW5516-3HA15<<",1795,"ST",1,"CP",1,"3RW44223BC35"]
["3RW4435-6BC36","SIRIUS soft starter Values at 575 V, 50 Β°C standard: 117 A, 100 hp Inside-delta: 203 A, 200 hp 400-690 V AC, 115 V AC Screw terminals !!! Phased-out product !!!  Successor is SIRIUS 3RW5,  Preferred successor type is >>3RW5535-6HA16<<",4627,"ST",1,"CP",1,"3RW44356BC36"]
["3RW4453-2BC36","SIRIUS soft starter Values at 575 V, 50 Β°C standard: 494 A, 500 hp Inside-delta: 856 A, 950 hp 400-690 V AC, 115 V AC spring-type terminals !!! Phased-out product !!! Successor is SIRIUS 3RW5, Preferred successor type is >>3RW5548-2HA16<<",14415,"ST",1,"CP",1,"3RW44532BC36"]
["3RW4776-0UB00","Enclosure base for 3RW40 Size S12",107,"ST",1,"CP",1,"3RW47760UB00"]
["3RW5056-2TB05","SIRIUS soft starter 200-600 V 171 A, 24 V AC/DC Spring-loaded terminals Thermistor input",2548,"ST",1,"CP",1,"3RW50562TB05"]
["3RW5076-2TB14","SIRIUS soft starter 200-480 V 470 A, 110-250 V AC Spring-loaded terminals Thermistor input",3604,"ST",1,"CP",1,"3RW50762TB14"]
["3RW5226-1TC15","SIRIUS soft starter 200-600 V 77 A, 110-250 V AC Screw terminals Thermistor input",1941,"ST",1,"CP",1,"3RW52261TC15"]
["3RW5244-2TC05","SIRIUS soft starter 200-600 V 250 A, 24 V AC/DC spring-type terminals Thermistor input",4528,"ST",1,"CP",1,"3RW52442TC05"]
["3RW5248-6AC14","SIRIUS soft starter 200-480 V 570 A, 110-250 V AC Screw terminals Analog output",7458,"ST",1,"CP",1,"3RW52486AC14"]
["3RW5536-2HA16","SIRIUS soft starter 200-690 V 171 A, 110-250 V AC spring-type terminals",5109,"ST",1,"CP",1,"3RW55362HA16"]
["3RW5545-6HA14","SIRIUS soft starter 200-480 V 315 A, 110-250 V AC Screw terminals",7392,"ST",1,"CP",1,"3RW55456HA14"]
["3RW5924-0SQ05","Power semiconductor module 600 V, for 3RW52/50, 315 A",588,"ST",1,"CP",1,"3RW59240SQ05"]
["3RW5954-0SN04","Power semiconductor module 480 V, for 3RW55, 210 A",588,"ST",1,"CP",1,"3RW59540SN04"]
["3RX9807-0AA00","Cable adapter EC for threaded joint, heavy gauge 13.5 AS-i cable connection to heavy-gauge threaded joint with insulation displacement system Continuation via standard cable",40,"ST",1,"CP",1,"3RX98070AA00"]
["3SB1901-3EE","Adhesive labeling plate on enclosure, Label size 22 x 22 mm, silver label, black font, with inscription: DOWN",5.8,"ST",1,"CP",10,"3SB19013EE"]
["3SB1901-4QE","Inscription plate for illuminated pushbutton and switch, flat, round, milky with black font, with graphic symbol: RELEASE BRAKE",237,"ST",1,"CP",10,"3SB19014QE"]
["3SB1904-2MK","Labeling plate for snapping on on label holder, Label size 17.5 x 28 mm, silver label, black font, with graphic symbol: 1 O 2 1 O 2",237,"ST",1,"CP",10,"3SB19042MK"]
["3SB2455-1E","Contact block and lampholder 1 NO, 1 NO, Wedge base W2 x 4.6 d, soldering pin connection",22.200000000000003,"ST",1,"CP",1,"3SB24551E"]
["3SB2901-4RF","Inscription plate for pushbutton and illuminated pushbutton flat, milky with black font, with graphic symbol: 5",87.1,"ST",100,"CP",10,"3SB29014RF"]
["3SB2908-1AF","incandescent lamp, clear, rated voltage 60 V AC/DC, 1.0 W, Wedge base W2 x 4.6 d,",2.93,"ST",1,"CP",10,"3SB29081AF"]
["3SB3000-2EA21","22MM PLASTIC ROUND ACTUATOR: SELECTOR SWITCH 3 SWITCH POSITIONS I-O-II MOMENTARY CONTACT TYPE NON-ILLUMINATED WITH HOLDER RED !!! Phased-out product !!! SIRIUS ACT 3SU1 is successor Preferred successor type is >>3SU1002-2BM20-0AA0 + 3SU1500-0AA10-0AA0<<",30.9,"ST",1,"CP",1,"3SB30002EA21"]
["3SB3000-5DD21","22MM PLASTIC ROUND ACTUATOR: BKS KEY-OPER.SWITCH WITH 2 KEYS 3 SWITCH POSITIONS I-O-II LATCHING LOCK NO S1, REMOVAL POS. I WITH HOLDER NOTE: BKS LOCKS E1 - E27 SUPPLIED WITHOUT KEYS !!! Phased-out product !!! SIRIUS ACT 3SU1 is successor Preferred successor type is >>3SU1000-5PL21-0AA0 + 3SU1500-0AA10-0AA0<<",174,"ST",1,"CP",1,"3SB30005DD21"]
["3SB3001-0DA41","22MM PLASTIC ROUND ACTUATOR: ILLUMINATED PUSHBUTTON WITH FLAT BUTTON LATCHING, UNLOCKING BY PRESSING AGAIN ILLUMINABLE INCL. HOLDER FOR 3 ELEMENTS WITH HOLDER GREEN !!! Phased-out product !!! SIRIUS ACT 3SU1 is successor Preferred successor type is >>3SU1001-0AA40-0AA0 +",33.300000000000004,"ST",1,"CP",1,"3SB30010DA41"]
["3SB3001-6CA70","22MM PLASTIC ROUND INDICATOR: INDICATOR LIGHT WITH SMOOTH LENSE ILLUMINABLE WITH HOLDER CLEAR",15.7,"ST",1,"CP",1,"3SB30016CA70"]
["3SB3201-0AA61-0CC0","22MM PLASTIC ROUND COMPLETE UNIT COMBINATION: PUSHBUTTON WITH FLAT BUTTON SPRING-LOADED TERMINAL, 1NO+1NC WITH HOLDER WHITE !!! Phased-out product !!! SIRIUS ACT 3SU1 is successor Preferred successor type is >>3SU1100-0AB60-3FA0<<",40.4,"ST",1,"CP",1,"3SB32010AA610CC0"]
["3SB3203-0AA21","22MM PLASTIC ROUND COMPLETE UNIT COMBINATION: PUSHBUTTON WITH FLAT BUTTON SCREW TERMINAL, 1NC WITH HOLDER RED !!! Phased-out product !!! SIRIUS ACT 3SU1 is successor Preferred successor type is >>3SU1100-0AB20-1CA0<<",30.5,"ST",1,"CP",1,"3SB32030AA21"]
["3SB3212-6AA60","22MM PLASTIC ROUND COMPLETE UNIT COMBINATION: INDICATOR LIGHT WITH SMOOTH LENSE ILLUMINATED WITH LAMP HOLDER BA 9S WITH LAMP 130V AC/DC SCREW TERMINAL OPERATIONAL VOLTAGE 220/230V AC WITH HOLDER WHITE !!! Phased-out product !!! SIRIUS ACT 3SU1 is successor Preferred successor type is >>3SU1106-6AA60-1AA0<<",48,"ST",1,"CP",1,"3SB32126AA60"]
["3SB3252-6AA50","22MM PLASTIC ROUND COMPLETE UNIT COMBINATION: INDICATOR LIGHT WITH SMOOTH LENSE ILLUMINATED WITH INTEGRATED LED 230V AC SCREW TERMINAL WITH HOLDER BLUE !!! Phased-out product !!! SIRIUS ACT 3SU1 is successor Preferred successor type is >>3SU1106-6AA50-1AA0<<",48.7,"ST",1,"CP",1,"3SB32526AA50"]
["3SB3304-6AA60","26X26MM PLASTIC SQUARE COMPLETE UNIT COMBINATION: INDICATOR LIGHT WITH SMOOTH LENSE NON-ILLUMINATED WITH LAMP HOLDER BA 9S WITHOUT LAMP SCREW TERMINAL WITH HOLDER WHITE !!! Phased-out product !!! SIRIUS ACT 3SU1 is successor Preferred successor type is >>3SU1001-6AA60-0AA0 + 3SU1500-0AA10-0AA0 + 3SU1900-0AX10-0AA0<<",27.700000000000003,"ST",1,"CP",1,"3SB33046AA60"]
["3SB3355-0AA31","Illuminated pushbutton, 26x26 mm, square, plastic, yellow, pushbutton, flat, 1NO + 1NC, lampholder, with integrated LED 230 V AC, SCREW TERMINAL !!! Phased-out product !!! SIRIUS ACT 3SU1 is the successor The preferred successor type is >>3SU1001-0AB30-0AA0 + 3SU1500-0AA10-0AA0 + 3SU1401-1BF30-1AA0 + 3SU1900-0AX10-0AA0 + 3SU1400-1AA10-1FA0<<",74.900000000000006,"ST",1,"CP",1,"3SB33550AA31"]
["3SB3420-0CA","COMPONENT FOR ENCLOSURE, 22MM CONTACT BLOCK WITH 1 CONTACT ELEMENT SCREW TERMINAL, 1NC GOLD-PLATED CONTACTS !!! Phased-out product !!! SIRIUS ACT 3SU1 is successor Preferred successor type is >>3SU1400-2AA10-1MA0<<",21.9,"ST",1,"CP",1,"3SB34200CA"]
["3SB3500-2DA51","22MM METAL ROUND ACTUATOR: SELECTOR SWITCH LATCHING 3 SWITCH POSITIONS I-O-II NON-ILLUMINATED WITH HOLDER BLUE !!! Phased-out product !!! SIRIUS ACT 3SU1 is successor Preferred successor type is >>3SU1002-2BL50-0AA0 + 3SU1500-0AA10-0AA0<<",33.9,"ST",1,"CP",1,"3SB35002DA51"]
["3SB3500-2QA41","22MM METAL ROUND ACTUATOR: SELECTOR SWITCH MOMENTARY CONTACT TYPE 2 SWITCH POSITIONS O-I NON-ILLUMINATED WITH HOLDER GREEN !!! Phased-out product !!! SIRIUS ACT 3SU1 is successor Preferred successor type is >>3SU1052-2BC40-0AA0 + 3SU1550-0AA10-0AA0<<",48.2,"ST",1,"CP",1,"3SB35002QA41"]
["3SB3500-4AD21","22MM ROUND METAL ACTUATOR: RONIS LOCK WITH 2 KEYS MAINTAINED CONTACT 2 SWITCH POSITIONS O-I LOCK NUMBER SB 30, REMOVE I WITH HOLDER POSSIBLE SPECIAL LOCKS FOR RONIS KEYSWITCHES: SB31, 455, 421 !!! Phased-out product !!! SIRIUS ACT 3SU1 is suc Preferred successor ty >>3SU1050-4BF21-0AA0 + 3SU1550-0AA10-0AA0<<",73.8,"ST",1,"CP",1,"3SB35004AD21"]
["3SB3500-5FD01","22MM METAL ROUND ACTUATOR: BKS KEY-OPER.SWITCH WITH 2 KEYS LEFT LATCH.,RI.MOMEN.CONT.TYPE 3 SWITCH POSITIONS I-O-II LOCK NO S1, REMOVAL POS. O WITH HOLDER NOTE: BKS LOCKS E1 - E27 SUPPLIED WITHOUT KEYS !!! Phased-out product !!! SIRIUS ACT 3SU1 is successor Preferred successor type is >>3SU1050-5PN01-0AA0 + 3SU1550-0AA10-0AA0<<",190,"ST",1,"CP",1,"3SB35005FD01"]
["3SB3501-2PA51","22MM METAL ROUND ACTUATOR: SELECTOR SWITCH HEAVY DUTY LATCHING 2 SWITCH POSITIONS O-I ILLUMINABLE WITH HOLDER BLUE !!! Phased-out product !!! SIRIUS ACT 3SU1 is successor Preferred successor type is >>3SU1052-2BF60-0AA0 + 3SU1550-0AA10-0AA0<<",53.4,"ST",1,"CP",1,"3SB35012PA51"]
["3SB3601-0AA41-0PA0","22MM METAL ROUND COMPLETE UNIT COMBINATION: PUSHBUTTON MOMENTARY CONTACT TYPE WITH FLAT BUTTON SCREW TERMINAL, 1NO+1NC WITH HOLDER GREEN !!! Phased-out product !!! SIRIUS ACT 3SU1 is successor Preferred successor type is >>3SU1150-0AB40-1FA0<<",39.300000000000004,"ST",1,"CP",1,"3SB36010AA410PA0"]
["3SB3608-2SA11","Selector switch, 22 mm, round, Metal, Black, Selector switch, short, heavy duty, 3 switch positions I-O-II, Latching, Actuating angle 2x50 degrees, With holder, 2 X 1NO+1NC, Screw terminal, Resistant to solvents !!! Phased-out product !!! Successor is SIRIUS ACT 3SU1 Preferred successor type is >>3SU1052-2BL10-0AA0 + 3SU1550-0AA10-0AA0 + 3SU1400-1AA10-1FA0<<",90,"ST",1,"CP",1,"3SB36082SA11"]
["3SB3647-0AA51-0PA0","22MM METAL ROUND COMPLETE UNIT COMBINATION: ILLUMINATED PUSHBUTTON MOMENTARY CONTACT TYPE WITH FLAT BUTTON ILLUMINATED WITH INTEGRATED LED 24V AC/DC SCREW TERMINAL, 1NO+1NC WITH HOLDER BLUE SOLVENT-RESISTANT NON INSCRIBABLE WITH LASER !!! Phased-out product !!! SIRIUS ACT 3SU1 is successor Preferred successor type is >>3SU1152-0AB50-1FA0<<",64.400000000000006,"ST",1,"CP",1,"3SB36470AA510PA0"]
["3SB3801-0DG3","Enclosure for command devices, 22mm, round, enclosure material plastic, enclosure top part yellow, 1 control point, A=Emergency stop mushroom pushbutton red, 40mm, rotate-to-unlatch, 1 NC, screw terminal, floor mounting, top and bottom 1 x M20 each !!! Phased-out product !!! Successor is SIRIUS ACT 3SU1",100,"ST",1,"CP",1,"3SB38010DG3"]
["3SB3901-0AL","ACCESSORY FOR ENCLOSURE, 22MM HEXAGON NUT FOR CABLE GLAND PG16 BLACK !!! Phased-out product !!! SIRIUS ACT 3SU1 is successor",302,"ST",1,"CP",10,"3SB39010AL"]
["3SB3903-0NJ","INSCRIPTION ACTUATOR/INDICATOR ON LABEL HOLDER INSCRIPTION LABEL FOR STICKING = BACKING PLATE LABEL SIZE 27 X 27 MM WITH GRAPHICAL SYMBOL: DIRECTION OF ARROW UPWARDS BLACK WITH WHITE PRINT",253,"ST",1,"CP",1,"3SB39030NJ"]
["3SB3905-1EL","INSCRIPTION ACTUATOR/INDICATOR ON LABEL HOLDER INSCRIPT.LABEL FOR SNAPPING ON = BACKING PLATE LABEL SIZE 17.5 X 28 MM WITH INSCRIPTION: START BLACK WITH WHITE PRINT !!! Phased-out product !!! SIRIUS ACT 3SU1 is successor Preferred successor type is >>3SU1900-0AD16-0DT0<<",185,"ST",1,"CP",10,"3SB39051EL"]
["3SB3906-1AJ","INSCRIPTION FOR ENCLOSURE INSCRIPTION LABEL FOR STICKING LABEL SIZE 22 X 22 MM WITH INSCRIPTION: LINKS BLACK WITH WHITE PRINT !!! Phased-out product !!! SIRIUS ACT 3SU1 is successor Preferred successor type is >>3SU1900-0AF16-0AJ0<<",4.55,"ST",1,"CP",10,"3SB39061AJ"]
["3SB3921-0BB","ACCESSORY / SPARE PART FOR PLASTIC-/METAL PROGRAM ROUND, 22MM: PROTECTIVE COLLAR FOR ANTI-ROTATION ELEMENT, 50.5MM YELLOW !!! Phased-out product !!! SIRIUS ACT 3SU1 is successor",25,"ST",1,"CP",1,"3SB39210BB"]
["3SE2100-0GW00-0AA3","METAL-ENCLOSED POSITION SWITCH POSITION SWITCH METAL-ENCLOSED 3XM20X1.5 SLOW-ACTION CONTACTS 1NO+1NC TWIST LEVER FINE ADJUSTMENT AND WITH STAINLESS STEEL ROLL",192,"ST",1,"CP",1,"3SE21000GW000AA3"]
["3SE2100-1W","POSITION SWITCH METAL-ENCLOSED",206,"ST",1,"CP",1,"3SE21001W"]
["3SE2120-1BV00-0AK0","POSITION SWITCH METAL-ENCLOSED, 1XM20X1.5 SNAP-ACTION CONTACTS 1NO+1NC SINGLE PLUNGER WITH INCR. CORROSION PROTECTION",172,"ST",1,"CP",1,"3SE21201BV000AK0"]
["3SE2120-1VW","METAL-ENCLOSED POSITION SWITCH, DEGREE OF PROTECTION IP67 SNAP-ACTION CONTACTS ALUMINUM ROD, 1 X M20 X 1.5",208,"ST",1,"CP",1,"3SE21201VW"]
["3SE2120-8GW00","POSITION SWITCH, METAL SNAP-ACTION CONTACTS 2NC, IP 67 TWIST LEVER, FINELY ADJUSTABLE POSITIVE OPENING, CABLE GLAND 1X (M20 X 1.5)",174,"ST",1,"CP",1,"3SE21208GW00"]
["3SE2200-1F","POSITION SWITCH, ENCLOSED IN MOULDED-PLASTIC HOUSING 30MM SNAP-ACTION CONTACTS 1NO+1NC, ANGULAR ROLLER LEVER",88.7,"ST",1,"CP",1,"3SE22001F"]
["3SE2200-8CV00","POS. SWITCH, MOULDED PLASTIC SNAP-ACTION CONTACTS 2NC, IP 67 ROUNDED PLUNGER POSITIVE OPENING, CABLE GLAND 1X (M20 X 1.5)",67.3,"ST",1,"CP",1,"3SE22008CV00"]
["3SE2303-1GW","METAL-ENCLOSED POSITION SWITCH, SLOW-ACTION CONTACTS 2NO+1NC, TWIST LEVER FINE ADJUSTMENT, 3 X M20 X 1.5",229,"ST",1,"CP",1,"3SE23031GW"]
["3SE2404-1EV00-0AA3","POSITION SWITCH METAL-ENCLOSED, ROLLER LEVER SNAP-ACTION CONTACTS 2NO+2NC 3XM20X1.5 WITH STAINLESS STEEL ROLL",346,"ST",1,"CP",1,"3SE24041EV000AA3"]
["3SE3003-0A","CONTACT BLOCK W. 3 CONTACTS F.POSITION SWITCHES SLOW-ACTION CONTACTS 1NO+2NC",101,"ST",1,"CP",1,"3SE30030A"]
["3SE3762-6XX00","POSITION SWITCH WITH TUMBLER MOULDED-PL., 5 DIR. OF APPROACH SPRING FORCE WITH AR (SEALABLE) 2NC/2NC, 110V AC",977,"ST",1,"CP",1,"3SE37626XX00"]
["3SE5000-0AV04","Separate actuator, radius actuator left for position switch with tumbler 3SE5312/3SE5322 and AS-i 3SF13 and position switch with separate actuator 3SE51/3SE52 and AS-i 3SF11/3SF12",28.400000000000002,"ST",1,"CP",1,"3SE50000AV04"]
["3SE5112-0KC02","Position switch Metal enclosure 40 mm according to EN 50041 Device connection 1x (M20 x 1.5) 1 NO/2 NC slow-action contacts Rounded plunger with 3 mm overtravel made of stainless steel",52,"ST",1,"CP",1,"3SE51120KC02"]
["3SE5114-0CH60-1AC5","Position switch, with Twist lever, adjustable-length with grid hole, Metal enclosure 40 mm according to EN 50041 1 NO/1 NC quick action contacts with M12 connector, 5-pole, fixed Pin assignment: Pin1=21, Pin2=22 Pin3=13, Pin4=14, Pin5=PE",90.399999999999991,"ST",1,"CP",1,"3SE51140CH601AC5"]
["3SE5132-0CJ80","Position switch Plastic enclosure 40 mm according to EN 50041 Device connection 1 x (M20 x 1.5) 1 NO/1 NC quick action contacts Rotary actuator right/left adjustable, Rod lever made of aluminum 200 mm long",43.2,"ST",1,"CP",1,"3SE51320CJ80"]
["3SE5162-0CB01","Position switch 3SE5162 Metal enclosure XL, 56 mm wide Plain plunger made of stainless steel Device connection 3 x (M20 x 1.5) 2 x (1 NO/1 NC) Quick action contacts IP66/IP67",90.899999999999991,"ST",1,"CP",1,"3SE51620CB01"]
["3SE5212-0PC05-1DA0","BASIC SWITCH FOR POSITION SWITCHES 3SE5112, ATEX METAL HOUSING 40MM WIDE, ACCORDING TO EN50041 DEVICE CONNECTION 1X (M20x1.5) 2S/ 1OE SLOW-ACTION CONTACTS WITHOUT ACTUATOR HEAD",77.3,"ST",1,"CP",1,"3SE52120PC051DA0"]
["3SE5232-0LD03","Position switch Plastic enclosure according to EN 50047, 31 mm Device connection 1 x (M20 x 1.5) 1 NO/2 NC quick action contacts Roller plunger, Form C with plastic roller 10 mm",26.5,"ST",1,"CP",1,"3SE52320LD03"]
["3SE5322-0SE22","Safety position switch with tumbler Locking force 1300 N 5 directions of approaches Spring-locked Auxiliary release with lock Magnet voltage 115 V AC Monitoring actuator 2 NC/1 NO Monitoring magnet 2 NC/1 NO Supplied without actuator. Actuator 3SE5000-0AV0. please order separately",250,"ST",1,"CP",1,"3SE53220SE22"]
["3SE5322-2SG22","Safety position switch with tumbler Locking force 1300 N 5 directions of approaches Spring-locked Escape release from the rear and auxiliary release on front Magnet voltage 115 V AC Monitoring actuator 2 NC/1 NO Monitoring magnet 2 NC/1 NO LED display yellow/green Supplied without actuator. Actuator 3SE5000-0AV0. please order separately",317,"ST",1,"CP",1,"3SE53222SG22"]
["3SE7140-1BD00-0AS0","Safety cable-operated switch Metal enclosure, Rope length 50m 2xM25x1.5; 1 NO/1 NC, Latching, only Bowden wire function, Pushbutton release, Red LED, 115 V",436,"ST",1,"CP",1,"3SE71401BD000AS0"]
["3SF3243-0XX40-0BA1","POSITION SWITCH WITH ASI-F-ADAPTER 2NC SLOW OPER. PERPENDICULAR TO AND ALONG AXIS,MOULD.PL., WIDTH 52 5N EXTRACTION FORCE WITHOUT ACTUATING ELEMENT",1112,"ST",1,"CP",1,"3SF32430XX400BA1"]
["3SK1122-2AB40","SIRIUS safety relay Basic unit Advanced series 3 electronic enabling circuits 1 electronic signaling circuit Us = 24 V DC Spring-type terminal (push-in)",198,"ST",1,"CP",1,"3SK11222AB40"]
["3SU1000-0CB20-0AA0","Pushbutton, 22 mm, round, plastic, red, Front ring, raised momentary contact type",7.25,"ST",1,"CP",1,"3SU10000CB200AA0"]
["3SU1000-5PC01-0AA0","Key-operated switch BKS, 22 mm, round, plastic, lock number S1, with 2 keys, 2 switch positions O<I, momentary contact type, Actuating angle 45Β°, 10:30h/12h, Key removal O",98,"ST",1,"CP",1,"3SU10005PC010AA0"]
["3SU1001-0AB30-0AA0","Illuminated pushbutton, 22 mm, round, plastic, yellow, pushbutton, flat momentary contact type",7,"ST",1,"CP",1,"3SU10010AB300AA0"]
["3SU1030-0AA50-0AA0","Pushbutton, 22 mm, round, plastic with metal front ring, blue, pushbutton, flat, latching, Push-to-release mechanism",25.8,"ST",1,"CP",1,"3SU10300AA500AA0"]
["3SU1030-3AB66-0AN0","Twin pushbutton, 22 mm, round, plastic with metal front ring, white: arrow pointing up, white: arrow pointing down, pushbuttons, flat",25.8,"ST",1,"CP",1,"3SU10303AB660AN0"]
["3SU1032-2BF10-0AA0","Selector switch, illuminable, 22 mm, round, plastic with metal front ring, black, selector switch, short, 2 switch positions O-I, latching, actuating angle 90Β°, 10:30h/13:30h",23.6,"ST",1,"CP",1,"3SU10322BF100AA0"]
["3SU1032-2BP30-0AA0","Selector switch, illuminable, 22 mm, round, plastic with metal front ring, yellow, selector switch, short, 3 switch positions I>O<II, momentary contact on the left, latching on the right, actuating angle 2x45Β°, 10:30h/12h/13:30h",24,"ST",1,"CP",1,"3SU10322BP300AA0"]
["3SU1050-4BL01-0AA0","RONIS key-operated switch, 22 mm, round, metal, shiny, lock number SB30, with 2 keys, 3 switch positions I-O-II, latching, actuating angle 2x45Β°, 10:30h/12h/13:30h, key removal O, possible special locks: SB31, 421, 455",31.200000000000003,"ST",1,"CP",1,"3SU10504BL010AA0"]
["3SU1050-5PN01-0AA0","Key-operated switch BKS, 22 mm, round, metal, shiny, lock number S1, with 2 keys, 3 switch positions I-O<II, left latching, right momentary contact type, actuating angle 2x45Β°, 10:30h/12h/13:30h, Key removal O",102,"ST",1,"CP",1,"3SU10505PN010AA0"]
["3SU1052-2CN60-0AA0","Selector switch, illuminable, 22 mm, round, metal, shiny, white, selector switch, long, 3 switch positions I-O<II, left latching, right momentary contact type, actuating angle 2x45Β°, 10:30h/12h/13:30h",16.900000000000002,"ST",1,"CP",1,"3SU10522CN600AA0"]
["3SU1062-2DF60-0AA0","Selector switch, illuminable, 30 mm, round, metal, matte, white, selector switch, short, front ring for flush installation, 2 switch positions O-I, latching, actuating angle 90Β°, 10:30h/13:30h",36.700000000000003,"ST",1,"CP",1,"3SU10622DF600AA0"]
["3SU1100-1HB20-1PG0","EMERGENCY STOP mushroom pushbutton, 22 mm, round, plastic, red, 40 mm, positive latching, acc. to EN ISO 13850, rotate-to-unlatch, with yellow backing plate, inscription: EMERGENCY STOP, with holder, 1 NC, 1 NC, screw terminal",43.6,"ST",1,"CP",1,"3SU11001HB201PG0"]
["3SU1106-0AB20-1FA0","Illuminated pushbutton, 22 mm, round, plastic, red, pushbutton, flat, momentary contact type, with holder, 1 NO+1 NC, LED module with integrated LED 230 V AC, screw terminal",33.800000000000004,"ST",1,"CP",1,"3SU11060AB201FA0"]
["3SU1132-0AB70-3FA0","Illuminated pushbutton, 22 mm, round, plastic with metal front ring, clear, pushbutton, flat, momentary contact type, with holder, 1 NO+1 NC, LED module with integrated LED 24 V AC/DC, Spring-type terminal",41.4,"ST",1,"CP",1,"3SU11320AB703FA0"]
["3SU1150-0AB50-1BA0","Pushbutton, 22 mm, round, metal, shiny, blue, pushbutton, flat, momentary contact type, 1 NO, screw terminal",17,"ST",1,"CP",1,"3SU11500AB501BA0"]
["3SU1152-0AB00-1BA0","Illuminated pushbutton, 22 mm, round, metal, shiny, amber, pushbutton, flat, momentary contact type, with holder, 1 NO, LED module with integrated LED 24 V AC/DC, screw terminal",26.8,"ST",1,"CP",1,"3SU11520AB001BA0"]
["3SU1250-2PS10-1AA0","Potentiometer, compact, 22 mm, round, metal, black, 10k ohm, with holder, screw terminal",119,"ST",1,"CP",1,"3SU12502PS101AA0"]
["3SU1400-1AA10-3BA0","Contact module with 1 contact element, 1 NO, spring-type terminal, for front plate mounting, Minimum order quantity 5 or a multiple thereof",5.33,"ST",1,"CP",5,"3SU14001AA103BA0"]
["3SU1401-1BB50-1AA2","LED module with integrated LED 24 V AC/DC, blue, screw terminal, for front plate mounting, ATEX Zone 1-2: Intrinsic safety",20.5,"ST",1,"CP",1,"3SU14011BB501AA2"]
["3SU1500-1AA10-1NA0","holder, 3-way, plastic, 1 NO, 1 NO, screw terminal",13,"ST",1,"CP",1,"3SU15001AA101NA0"]
["3SU1801-0AP00-4NB1","Enclosure for command devices 22 mm, round, enclosure material plastic, enclosure top part gray, 1 control point, plastic, A=Illuminated pushbutton yellow, momentary contact type, 40 mm, 1 NO, spring-type terminal,  LED module yellow, floor mounting, wired, recess for label, at bottom M12 connector 5-pole",121,"ST",1,"CP",1,"3SU18010AP004NB1"]
["3SU1804-0AA00-0AB1","Enclosure for command devices, 22 mm, round, Enclosure material plastic, enclosure top part gray, 4 control points plastic, Recess for labels, without equipment",22.5,"ST",1,"CP",1,"3SU18040AA000AB1"]
["3SU1900-0AB71-0QT0","Inscription plate for illuminated pushbutton, round, milky with black font, with graphic symbol: rotation to the right",147,"ST",100,"CP",10,"3SU19000AB710QT0"]
["3SU1900-0AC81-0DY0","Labeling plate for snapping on or gluing, on label holder, label size 12.5x27 mm, silver label, black font with inscription: Man O Auto",147,"ST",100,"CP",10,"3SU19000AC810DY0"]
["3SU1900-0AD81-0QB0","Labeling plate for snapping on or gluing on label holder, Label size 17.5 x 27 mm, silver label, black font, with graphic symbol: I",147,"ST",100,"CP",10,"3SU19000AD810QB0"]
["3SU1900-0AF16-0AH0","Labeling plate for gluing on enclosure, label size 22x22 mm, black label, white font, with inscription: Rechts",3.67,"ST",1,"CP",10,"3SU19000AF160AH0"]
["3SU1900-0AF81-0DS0","Labeling plate for gluing on enclosure, label size 22x22mm, silver label, black font, with inscription: Stop",3.47,"ST",1,"CP",10,"3SU19000AF810DS0"]
["3SU1901-0BD31-0AT0","Washer round for EMERGENCY STOP mushroom pushbutton, yellow, illuminated, thickness 5 mm, outer diameter 60 mm, inside diameter 23 mm, with inscription: NOT-HALT",120,"ST",1,"CP",10,"3SU19010BD310AT0"]
["3SU1960-0EY70-0AA0","Sealable cap for selector switch, short, 30 mm, clear",32.6,"ST",1,"CP",1,"3SU19600EY700AA0"]
["3SX3271","TWIST LEVER (FINE ADJUSTABLE) FROM 10 TO 10 DEG. W. STAINLESS STEEL ROLLER FOR 3SE.200 AND 3SE.210",37.200000000000003,"ST",1,"CP",1,"3SX3271"]
["3TB5017-0LV4","Contactor, size 6, 3-pole, AC-3, 55 kW, 400 / 380 V Auxiliary contacts 21 (2 NO + 1 NC) 36 V DC DC operation connected to varistor Operating range 0.7 to 1.25 x US !!! Phased-out product !!! Successor is SIRIUS 3RT",1607,"ST",1,"CP",1,"3TB50170LV4"]
["3TC4417-0BR2","Contactor, Size 2, 2-pole, DC-3 and 5, 32 A Auxiliary contacts 22 (2 NO + 2 NC) 440 V AC 50/60 Hz AC operation",229,"ST",1,"CP",1,"3TC44170BR2"]
["3TC5217-0AE4","Contactor, Size 8, 2-pole, DC-3 and 5, 220 A Auxiliary switch 22 (2 NO + 2 NC) 60 V DC DC operation",1808,"ST",1,"CP",1,"3TC52170AE4"]
["3TF2010-0AK6","Contactor, Size 00, 3-pole, AC-3 4 kW/400 V; Screw terminal Auxiliary switch 10E (1 NO) 120 V AC 60 Hz/110 V AC 50 Hz AC operation !!! Phased-out product !!! Successor is SIRIUS 3RT201 or 3TG10",62,"ST",1,"CP",1,"3TF20100AK6"]
["3TF2801-0BB4","Contactor, Size 00, 3-pole, AC-3 2.2 kW/400 V, Screw terminal Auxiliary switch 01E (1 NC) 24 VDC DC operation !!! Phased-out product !!! Successor is SIRIUS 3RT201 or 3TG10",67.699999999999989,"ST",1,"CP",1,"3TF28010BB4"]
["3TF6844-0CP70-0B","Vacuum contactor, ABB V 630-30-44 Contactor, Size 14, 3-pole AC-3, 335kW, 400/380 V (690 V) Auxiliary switch 44 (4NO+4NC) AC operation 230...276 V AC 50/60 Hz",5085,"ST",1,"CP","On request","3TF68440CP700B"]
["3TH2022-0AK1","Contactor relay, 22E, EN 50011, 2 NO + 2 NC, Screw terminal AC operation 120 V AC 60 Hz/100 V AC 50 Hz !!! Phased-out product !!! Successor is SIRIUS 3RH21",66.399999999999991,"ST",1,"CP",1,"3TH20220AK1"]
["3TH2040-0BD4","Contactor relay 40 E EN 50011 4 NO;Screw terminal Direct current operation 42 V DC !!! Phased-out product !!! Successor is SIRIUS 3RH21",75.899999999999991,"ST",1,"CP",1,"3TH20400BD4"]
["3TH2171-0BB4","Contactor relay, 71E, EN 50011, 7 NO + 1 NC; Screw terminal Width 90 mm 24 V DC DC operation !!! Phased-out product !!! Successor is SIRIUS 3RH21",111,"ST",1,"CP",1,"3TH21710BB4"]
["3TH4244-0LB4","Contactor relay, 44E, DIN EN 50011, for railway applications 4NO+4NC, screw terminal Operating range 0.7...1.25xUS connected to varistor 24 V DC",146,"ST",1,"CP",1,"3TH42440LB4"]
["3TH4271-0AB0","Contactor relay, 71E, DIN EN 50011, 7 NO + 1 NC, screw terminal AC operation 24 V AC 50 Hz/29 V AC 60 Hz",75.5,"ST",1,"CP",1,"3TH42710AB0"]
["3TH4310-0BG4","Contactor relay, 100E, EN 50011 10 NO, screw terminal, DC operation, 125 V DC",180,"ST",1,"CP",1,"3TH43100BG4"]
["3TH4355-4MP0","Contactor relay, 55E, EN 50011, 5NO + 5NC flat connector terminal AC operation 230 V AC 50 Hz, 277 V 60 Hz",154,"ST",1,"CP",1,"3TH43554MP0"]
["3TH4382-0AJ2","Contactor relay, 82E, EN 50011, 8 NO + 2 NC, screw terminal, AC operation, 115 V AC 50/60 Hz",143,"ST",1,"CP",1,"3TH43820AJ2"]
["3TK2022-7BM4","Miniature contactor, Flat connector terminal 2 NO + 2 NC Screw mounting (diagonal) 220 V DC DC operation !!! Phased-out product !!! Successor is SIRIUS 3RT23/25",63.2,"ST",1,"CP",1,"3TK20227BM4"]
["3TK2810-1KA42-0AA0","SIRIUS safety relay Safety-oriented Speed monitoring 110-240 V AC/DC, 45 mm overall width Spring-type terminal EC instantaneous: 2 NO EC delayed: 0 SC: 2 electrical NAMUR version Auto-start/manual start Basic device Maximum achievable PL according to EN 13849-1: e Maximum achievable SIL according to IEC 61508: 3",1918,"ST",1,"CP",1,"3TK28101KA420AA0"]
["3TK2826-0DA00-0HA0","!!! Phased-out product !!! The successor product is 3ZY1321-2AA00 for 3SK SIRIUS safety relay Sealable cover cap for 3TK2826",8.65,"ST",1,"CP",5,"3TK28260DA000HA0"]
["3TK2840-2BB40","SIRIUS safety relay with electronic enabling circuits (EC) 24 V DC, 22.5 mm Spring-type terminal EC instantaneous: 2 HL EC delayed: 0 SC: 0 Autostart/monitored start Base unit Maximum achieved SIL: 2, PL: d",291,"ST",1,"CP",1,"3TK28402BB40"]
["3TX5903-0AL0","Accessories for 3TM latching system for retrofitting shunt release AC 100V",1552,"ST",1,"LP",1,"3TX59030AL0"]
["3TX7402-3A","Surge suppressor Interference suppression diode with cable spacer 24-250 V DC for mounting to coil terminal for contactor relays 3TH4",12.7,"ST",1,"CP",1,"3TX74023A"]
["3TX7522-3R","Surge suppressor RC element for snapping on 24-48 V AC / 24-70 V DC for contactors Size 8-12, AC operation Size 3-6, DC operation",55.9,"ST",1,"CP",1,"3TX75223R"]
["3TY5656-0AS2","Magnet Coil and Resistor for contactor 3TL6 AC 50/60Hz, 575V",2599,"ST",1,"LP",1,"3TY56560AS2"]
["3TY5812-0DA0","Electr. module f. controling of magnet coil for contactor 3TL8 operating voltage AC/DC 48V-60V","On Request","ST",1,"LP",1,"3TY58120DA0"]
["3TY6443-0LF4","Magnet coil for contactors 3TC44 with series resistor without varistor 110 V DC",102,"ST",1,"CP",1,"3TY64430LF4"]
["3TY7503-0AU1","Magnet coil for contactors 3TF50/51 and 3TK50 277 V AC 60 Hz",112,"ST",1,"CP",1,"3TY75030AU1"]
["3TY7543-0DW4","Magnet coil for contactors 3TF54/55 and 3TK54 DC economy circuit 48 V DC",282,"ST",1,"CP",1,"3TY75430DW4"]
["3TY7573-0DP4","Magnet coil for contactors 3TF57 SPU 230 V-190.4-210.4 ohm",358,"ST",1,"CP",1,"3TY75730DP4"]
["3UA7021-0E","Overload relay for mounting to contactor 0.25...0.4 A, 1 NO + 1 NC",132,"ST",1,"CP",1,"3UA70210E"]
["3UF5031-3BB10-1","SIMOCODE DP basic unit PROFIBUS DP interface 1.5 Mbaud, RS485 4I/4O freely parameterizable US: 24 V DC 50...205 A, overall width 120 mm Input for summation current transformer for ground fault detection Bistable outputs",6354,"ST",1,"CP",1,"3UF50313BB101"]
["3UG4512-1AR20","Analog monitoring relay Phase failure and sequence 3 x 160...690 V 50...60 Hz AC 1 change-over contact screw terminal",95.899999999999991,"ST",1,"CP",1,"3UG45121AR20"]
["3UG4633-1AL30","Digital monitoring relay Voltage monitoring, 22.5 mm from 17-275 V AC/DC Overshoot and undershoot Self-powered Spike delay 0.1 to 20 s Hysteresis 0.1 to 150 V 1 CO contact With or without error buffer Screw terminals Successor product for 3UG3534, 3UG3535",142,"ST",1,"CP",1,"3UG46331AL30"]
["3VA1010-3ED32-0HA0","Circuit breaker 3VA1 IEC Frame 100 Switching capacity class N Icu=25 kA @ 415 V 3-pole, system protection TM210, FTFM, In=100 A Overload protection Ir=100 A non-adjustable short-circuit protection Ii = 10 x In Lug terminal Shunt release (STL) 12-30 V DC, 24 V AC 50/60 Hz",226,"ST",1,"LP",1,"3VA10103ED320HA0"]
["3VA1010-4ED32-0KA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=100A overload protection Ir=100A fixed short-circuit protection Ii=10 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC",240,"ST",1,"LP",1,"3VA10104ED320KA0"]
["3VA1020-2ED32-0AC0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 3-pole, line protection TM210, FTFM, In=20A overload protection Ir=20A fixed short-circuit protection Ii=16 x In nut keeper kit 2 auxiliary switches HQ",175,"ST",1,"LP",1,"3VA10202ED320AC0"]
["3VA1020-3ED36-0AD0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM210, FTFM, In=20A overload protection Ir=20A fixed short-circuit protection Ii=16 x In clamp connection 3 auxiliary switches HQ",210,"ST",1,"LP",1,"3VA10203ED360AD0"]
["3VA1032-2ED32-0HH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 3-pole, line protection TM210, FTFM, In=32A overload protection Ir=32A fixed short-circuit protection Ii=10 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",255,"ST",1,"LP",1,"3VA10322ED320HH0"]
["3VA1032-4ED32-0HC0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=32A overload protection Ir=32A fixed short-circuit protection Ii=10 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ",242,"ST",1,"LP",1,"3VA10324ED320HC0"]
["3VA1032-4ED36-0KH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=32A overload protection Ir=32A fixed short-circuit protection Ii=10 x In clamp connection shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ",277,"ST",1,"LP",1,"3VA10324ED360KH0"]
["3VA1040-4ED32-0AA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=40A overload protection Ir=40A fixed short-circuit protection Ii=10 x In nut keeper kit",144,"ST",1,"LP",1,"3VA10404ED320AA0"]
["3VA1050-4ED32-0AE0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=50A overload protection Ir=50A fixed short-circuit protection Ii=10 x In nut keeper kit 4 auxiliary switches HQ",215,"ST",1,"LP",1,"3VA10504ED320AE0"]
["3VA1050-4ED42-0AH0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM210, FTFM, In=50A overload protection Ir=50A fixed short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit 2 auxiliary switches HQ 1 trip alarm switch HQ",240,"ST",1,"LP",1,"3VA10504ED420AH0"]
["3VA1063-2ED42-0DA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 4-pole, line protection TM210, FTFM, In=63A overload protection Ir=63A fixed short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz",262,"ST",1,"LP",1,"3VA10632ED420DA0"]
["3VA1063-4ED42-0CC0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM210, FTFM, In=63A overload protection Ir=63A fixed short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ",305,"ST",1,"LP",1,"3VA10634ED420CC0"]
["3VA1080-2ED36-0DC0","circuit breaker 3VA1 IEC frame 100 breaking capacity class B Icu=16kA @ 415V 3-pole, line protection TM210, FTFM, In=80A overload protection Ir=80A fixed short-circuit protection Ii=10 x In clamp connection undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",286,"ST",1,"LP",1,"3VA10802ED360DC0"]
["3VA1080-3ED36-0JC0","circuit breaker 3VA1 IEC frame 100 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM210, FTFM, In=80A overload protection Ir=80A fixed short-circuit protection Ii=10 x In clamp connection shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",269,"ST",1,"LP",1,"3VA10803ED360JC0"]
["3VA1080-4ED42-0AD0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM210, FTFM, In=80A overload protection Ir=80A fixed short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit 3 auxiliary switches HQ",258,"ST",1,"LP",1,"3VA10804ED420AD0"]
["3VA1096-4ED32-0HA0","circuit breaker 3VA1 IEC frame 100 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM210, FTFM, In=16A overload protection Ir=16A fixed short-circuit protection Ii=10 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz",208,"ST",1,"LP",1,"3VA10964ED320HA0"]
["3VA1110-3EF32-0CC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ",317,"ST",1,"LP",1,"3VA11103EF320CC0"]
["3VA1110-4EF32-0BC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ",335,"ST",1,"LP",1,"3VA11104EF320BC0"]
["3VA1110-5EF32-0CH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",375,"ST",1,"LP",1,"3VA11105EF320CH0"]
["3VA1110-5MH36-0AF0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, starter protection TM120M, AM, In=100A without overload protection short-circuit protection Ii=5...15 x In clamp connection 1 auxiliary switch HQ 1 trip alarm switch HQ",292,"ST",1,"LP",1,"3VA11105MH360AF0"]
["3VA1110-6EF36-0JH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=100A overload protection Ir=70A...100A short-circuit protection Ii=5...10 x In clamp connection shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",395,"ST",1,"LP",1,"3VA11106EF360JH0"]
["3VA1112-1AA42-0HH0","switch disconnector 3VA1 IEC frame 160 4-pole SD100, In=125A without overload protection w/o short-circuit protection nut keeper kit shunt trip (STL) 12-30V DC; 24 V AC 50/60 Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",392,"ST",1,"LP",1,"3VA11121AA420HH0"]
["3VA1112-3EF36-0AB0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=125A overload protection Ir=88A...125A short-circuit protection Ii=5...10 x In clamp connection 2 auxiliary switches HP",352,"ST",1,"LP",1,"3VA11123EF360AB0"]
["3VA1112-4GD42-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM210, FTFM, In=125A overload protection Ir=125A fixed short-circuit protection Ii=10 x In N conductor protection 100% nut keeper kit",428,"ST",1,"LP",1,"3VA11124GD420AA0"]
["3VA1112-5EF32-0AB0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=125A overload protection Ir=88A...125A short-circuit protection Ii=5...10 x In nut keeper kit 2 auxiliary switches HP",410,"ST",1,"LP",1,"3VA11125EF320AB0"]
["3VA1112-5MH32-0KA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, starter protection TM120M, AM, In=125A without overload protection short-circuit protection Ii=5...15 x In nut keeper kit shunt trip (STL) 220-250 V DC; 208-277 V AC",452,"ST",1,"LP",1,"3VA11125MH320KA0"]
["3VA1112-6MH36-0AE0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, starter protection TM120M, AM, In=125A without overload protection short-circuit protection Ii=5...15 x In clamp connection 4 auxiliary switches HQ",511,"ST",1,"LP",1,"3VA11126MH360AE0"]
["3VA1116-1AA42-0AH0","switch disconnector 3VA1 IEC frame 160 4-pole SD100, In=160A without overload protection w/o short-circuit protection nut keeper kit 2 auxiliary switches HQ 1 trip alarm switch HQ",348,"ST",1,"LP",1,"3VA11161AA420AH0"]
["3VA1116-4EF32-0CA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz",390,"ST",1,"LP",1,"3VA11164EF320CA0"]
["3VA1116-5ED42-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM210, FTFM, In=160A overload protection Ir=160A fixed short-circuit protection Ii=10 x In N conductor unprotected nut keeper kit",489,"ST",1,"LP",1,"3VA11165ED420AA0"]
["3VA1116-5EF36-0DA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In clamp connection undervoltage release (UVR) 208-230V AC 50/60Hz",454,"ST",1,"LP",1,"3VA11165EF360DA0"]
["3VA1116-6EF32-0CH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",518,"ST",1,"LP",1,"3VA11166EF320CH0"]
["3VA1120-3EF36-0DH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=20A overload protection Ir=14A...20A short-circuit protection Ii=8...16 x In clamp connection undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",309,"ST",1,"LP",1,"3VA11203EF360DH0"]
["3VA1120-5EF32-0DA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=20A overload protection Ir=14A...20A short-circuit protection Ii=8...16 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz",273,"ST",1,"LP",1,"3VA11205EF320DA0"]
["3VA1120-6ED36-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM210, FTFM, In=20A overload protection Ir=20A fixed short-circuit protection Ii=16 x In clamp connection",209,"ST",1,"LP",1,"3VA11206ED360AA0"]
["3VA1125-3EF32-0AH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=25A overload protection Ir=18A...25A short-circuit protection Ii=6.4...12.8 x In nut keeper kit 2 auxiliary switches HQ 1 trip alarm switch HQ",211,"ST",1,"LP",1,"3VA11253EF320AH0"]
["3VA1125-6EF32-0BH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=25A overload protection Ir=18A...25A short-circuit protection Ii=6.4...12.8 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ",341,"ST",1,"LP",1,"3VA11256EF320BH0"]
["3VA1132-3EF32-0BH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=32A overload protection Ir=22A...32A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ",293,"ST",1,"LP",1,"3VA11323EF320BH0"]
["3VA1132-5ED46-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM210, FTFM, In=32A overload protection Ir=32A fixed short-circuit protection Ii=10 x In N conductor unprotected clamp connection",252,"ST",1,"LP",1,"3VA11325ED460AA0"]
["3VA1132-5EF32-0KA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=32A overload protection Ir=22A...32A short-circuit protection Ii=5...10 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC",253,"ST",1,"LP",1,"3VA11325EF320KA0"]
["3VA1140-3EF32-0HH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=40A overload protection Ir=28A...40A short-circuit protection Ii=5...10 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",275,"ST",1,"LP",1,"3VA11403EF320HH0"]
["3VA1140-4EF36-0AB0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=40A overload protection Ir=28A...40A short-circuit protection Ii=5...10 x In clamp connection 2 auxiliary switches HP",241,"ST",1,"LP",1,"3VA11404EF360AB0"]
["3VA1140-5GE46-0AA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM220, ATFM, In=40A overload protection Ir=28A...40A short-circuit protection Ii=10 x In N conductor protection 100% clamp connection",256,"ST",1,"LP",1,"3VA11405GE460AA0"]
["3VA1150-3EF36-0AG0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=50A overload protection Ir=35A...50A short-circuit protection Ii=5...10 x In clamp connection 1 auxiliary switch HP 1 trip alarm switch HP",229,"ST",1,"LP",1,"3VA11503EF360AG0"]
["3VA1150-4EF36-0DC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=50A overload protection Ir=35A...50A short-circuit protection Ii=5...10 x In clamp connection undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",306,"ST",1,"LP",1,"3VA11504EF360DC0"]
["3VA1150-5EF32-0JC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=50A overload protection Ir=35A...50A short-circuit protection Ii=5...10 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",288,"ST",1,"LP",1,"3VA11505EF320JC0"]
["3VA1150-6EF36-0AC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=50A overload protection Ir=35A...50A short-circuit protection Ii=5...10 x In clamp connection 2 auxiliary switches HQ",258,"ST",1,"LP",1,"3VA11506EF360AC0"]
["3VA1163-3EF32-0DH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=63A overload protection Ir=44A...63A short-circuit protection Ii=5...10 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",293,"ST",1,"LP",1,"3VA11633EF320DH0"]
["3VA1163-5ED32-0BA0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM210, FTFM, In=63A overload protection Ir=63A fixed short-circuit protection Ii=10 x In nut keeper kit undervoltage release (UVR) 24V DC",258,"ST",1,"LP",1,"3VA11635ED320BA0"]
["3VA1163-5EE32-0BH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM220, ATFM, In=63A overload protection Ir=44A...63A short-circuit protection Ii=10 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ",315,"ST",1,"LP",1,"3VA11635EE320BH0"]
["3VA1163-6EF32-0AC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=63A overload protection Ir=44A...63A short-circuit protection Ii=5...10 x In nut keeper kit 2 auxiliary switches HQ",241,"ST",1,"LP",1,"3VA11636EF320AC0"]
["3VA1163-6MH32-0JH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, starter protection TM120M, AM, In=63A without overload protection short-circuit protection Ii=5...15 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",323,"ST",1,"LP",1,"3VA11636MH320JH0"]
["3VA1180-3EF32-0JC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=80A overload protection Ir=56A...80A short-circuit protection Ii=5...10 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ",245,"ST",1,"LP",1,"3VA11803EF320JC0"]
["3VA1180-5EF36-0AF0","circuit breaker 3VA1 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=80A overload protection Ir=56A...80A short-circuit protection Ii=5...10 x In clamp connection 1 auxiliary switch HQ 1 trip alarm switch HQ",259,"ST",1,"LP",1,"3VA11805EF360AF0"]
["3VA1180-6EF36-0DH0","circuit breaker 3VA1 IEC frame 160 breaking capacity class H Icu=70kA @ 415V 3-pole, line protection TM240, ATAM, In=80A overload protection Ir=56A...80A short-circuit protection Ii=5...10 x In clamp connection undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",378,"ST",1,"LP",1,"3VA11806EF360DH0"]
["3VA1196-3EF32-0AF0","circuit breaker 3VA1 IEC frame 160 breaking capacity class N Icu=25kA @ 415V 3-pole, line protection TM240, ATAM, In=16A overload protection Ir=11A...16A short-circuit protection Ii=10...20 x In nut keeper kit 1 auxiliary switch HQ 1 trip alarm switch HQ",195,"ST",1,"LP",1,"3VA11963EF320AF0"]
["3VA1196-4EF36-0CC0","circuit breaker 3VA1 IEC frame 160 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=16A overload protection Ir=11A...16A short-circuit protection Ii=10...20 x In clamp connection undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ",306,"ST",1,"LP",1,"3VA11964EF360CC0"]
["3VA1216-5EF32-0AD0","circuit breaker 3VA1 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=160A overload protection Ir=112A...160A short-circuit protection Ii=5...10 x In nut keeper kit 3 auxiliary switches HQ",499,"ST",1,"LP",1,"3VA12165EF320AD0"]
["3VA1220-4EF42-0AA0","circuit breaker 3VA1 IEC frame 250 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM240, ATAM, In=200A overload protection Ir=140A...200A short-circuit protection Ii=5...10 x In N conductor unprotected nut keeper kit",553,"ST",1,"LP",1,"3VA12204EF420AA0"]
["3VA1220-4GF42-0AJ0","circuit breaker 3VA1 IEC frame 250 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM240, ATAM, In=200A overload protection Ir=140A...200A short-circuit protection Ii=5...10 x In N conductor protection 100% nut keeper kit 2 auxiliary switches HP 1 trip alarm switch HP",749,"ST",1,"LP",1,"3VA12204GF420AJ0"]
["3VA1220-5GF42-0AA0","circuit breaker 3VA1 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection TM240, ATAM, In=200A overload protection Ir=140A...200A short-circuit protection Ii=5...10 x In N conductor protection 100% nut keeper kit",743,"ST",1,"LP",1,"3VA12205GF420AA0"]
["3VA1225-1AA32-0AB0","switch disconnector 3VA1 IEC frame 250 3-pole SD100, In=250A without overload protection w/o short-circuit protection nut keeper kit 2 auxiliary switches HP",430,"ST",1,"LP",1,"3VA12251AA320AB0"]
["3VA1225-4EF32-0AA0","circuit breaker 3VA1 IEC frame 250 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=250A overload protection Ir=175A...250A short-circuit protection Ii=5...10 x In nut keeper kit",416,"ST",1,"LP",1,"3VA12254EF320AA0"]
["3VA1225-4GF42-0AG0","circuit breaker 3VA1 IEC frame 250 breaking capacity class S Icu=36kA @ 415V 4-pole, line protection TM240, ATAM, In=250A overload protection Ir=175A...250A short-circuit protection Ii=5...10 x In N conductor protection 100% nut keeper kit 1 auxiliary switch HP 1 trip alarm switch HP",808,"ST",1,"LP",1,"3VA12254GF420AG0"]
["3VA1225-6EF42-0CH0","circuit breaker 3VA1 IEC frame 250 breaking capacity class H Icu=70kA @ 415V 4-pole, line protection TM240, ATAM, In=250A overload protection Ir=175A...250A short-circuit protection Ii=5...10 x In N conductor unprotected nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",662,"ST",1,"LP",1,"3VA12256EF420CH0"]
["3VA1225-6FF42-0AA0","circuit breaker 3VA1 IEC frame 250 breaking capacity class H Icu=70kA @ 415V 4-pole, line protection TM240, ATAM, In=250A overload protection Ir=175A...250A short-circuit protection Ii=5...10 x In N conductor protection 50% nut keeper kit",843,"ST",1,"LP",1,"3VA12256FF420AA0"]
["3VA1340-5EF32-0DH0","circuit breaker 3VA1 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=400A overload protection Ir=280A...400A short-circuit protection Ii=5...10 x In nut keeper kit circuit breaker 3VA1 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=400A overload protection Ir=280A...400A short-circuit protection Ii=5...10 x In nut UNDERVOLTAGE RELEASE 208-230 V AC 50/60 HZ ACCESSORY FOR 3VA1 2 AUXILIARY SWITCH CHANGEOVER H 1 TRIP ALARM SWITCH CHANGEOVER",1016,"ST",1,"LP",1,"3VA13405EF320DH0"]
["3VA1463-4EF32-0KB0","circuit breaker 3VA1 IEC frame 630 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=630A overload protection Ir=440A...630A short-circuit protection Ii=4...8 x In nut keeper kit circuit breaker 3VA1 IEC frame 630 breaking capacity class S Icu=36kA @ 415V 3-pole, line protection TM240, ATAM, In=630A overload protection Ir=440A...630A short-circuit protection Ii=4...8 x In nut SHUNT TRIP LEFT 208-277 V AC 50/60 HZ 220-250 V DC ACCESSORY 2 AUXILIARY SWITCH CHANGEOVER H",1254,"ST",1,"LP",1,"3VA14634EF320KB0"]
["3VA1580-5EF32-0JL0","circuit breaker 3VA1 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection TM240, ATAM, In=800A overload protection Ir=560A...800A short-circuit protection Ii=5 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",1895,"ST",1,"LP",1,"3VA15805EF320JL0"]
["3VA2010-5HN32-0CL0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",562,"ST",1,"LP",1,"3VA20105HN320CL0"]
["3VA2010-5HN36-0JH0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In clamp connection shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",537,"ST",1,"LP",1,"3VA20105HN360JH0"]
["3VA2010-6HN32-0BL0","circuit breaker 3VA2 IEC frame 100 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",608,"ST",1,"LP",1,"3VA20106HN320BL0"]
["3VA2010-6JQ32-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU560, LSIG, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit",821,"ST",1,"LP",1,"3VA20106JQ320AA0"]
["3VA2025-5KP42-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU850, LSI, In=25A overload protection Ir=10A...25A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) nut keeper kit",816,"ST",1,"LP",1,"3VA20255KP420AA0"]
["3VA2040-6JQ46-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class H Icu=85kA @ 415V 4-pole, line protection ETU560, LSIG, In=40A overload protection Ir=16A...40A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) gr.-fault prot., can be sw. off Ig=0.4...1 x In= tg=0.05-0.8s clamp connection",903,"ST",1,"LP",1,"3VA20406JQ460AA0"]
["3VA2040-7HL32-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU320, LI, In=40A overload protection Ir=16A...40A short-circuit protection Ii=1.5...12 x In nut keeper kit",402,"ST",1,"LP",1,"3VA20407HL320AA0"]
["3VA2063-5HL36-0JL0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=63A overload protection Ir=25A...63A short-circuit protection Ii=1.5...12 x In clamp connection shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",494,"ST",1,"LP",1,"3VA20635HL360JL0"]
["3VA2063-5HN42-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU350, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In N conductor protection adjustable (OFF, 100%) nut keeper kit",468,"ST",1,"LP",1,"3VA20635HN420AA0"]
["3VA2063-5KQ42-0AA0","circuit breaker 3VA2 IEC frame 100 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU860, LSIG, In=63A overload protection Ir=25A...63A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) gr.-fault prot., can be sw. off Ig=0.25...1 x In= tg=0.05-0.8s nut keeper kit",898,"ST",1,"LP",1,"3VA20635KQ420AA0"]
["3VA2110-0MQ32-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class  E Icu=200 kA @ 415 V 3-pole motor protection ETU860M,  LSIG, In=100A overload protection Ir=40A ... 100A short circuit protection Isd=1,2...15xIn, Ii=3...15xIn busbar connection",866,"ST",1,"LP",1,"3VA21100MQ320AA0"]
["3VA2110-5HL36-0BA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=100A overload protection Ir=40A...100A short-circuit protection Ii=1.5...12 x In clamp connection undervoltage release (UVR) 24V DC",461,"ST",1,"LP",1,"3VA21105HL360BA0"]
["3VA2110-5JQ32-0AF0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU560, LSIG, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit 1 auxiliary switch HQ 1 trip alarm switch HQ",811,"ST",1,"LP",1,"3VA21105JQ320AF0"]
["3VA2110-5KP32-0KA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU850, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer nut keeper kit shunt trip (STL) 220-250V DC; 208-277V AC",806,"ST",1,"LP",1,"3VA21105KP320KA0"]
["3VA2110-6HL32-0CH0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU320, LI, In=100A overload protection Ir=40A...100A short-circuit protection Ii=1.5...12 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",538,"ST",1,"LP",1,"3VA21106HL320CH0"]
["3VA2110-6HN32-0HC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ",545,"ST",1,"LP",1,"3VA21106HN320HC0"]
["3VA2110-7MN32-0AJ0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 3-pole, motor protection ETU350M, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit 2 auxiliary switches HP 1 trip alarm switch HP",529,"ST",1,"LP",1,"3VA21107MN320AJ0"]
["3VA2110-8KP36-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class L Icu=150kA @ 415V 3-pole, line protection ETU850, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% clamp connection",883,"ST",1,"LP",1,"3VA21108KP360AA0"]
["3VA2116-5HL32-0DC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=160A overload protection Ir=63A...160A short-circuit protection Ii=1.5...10 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",667,"ST",1,"LP",1,"3VA21165HL320DC0"]
["3VA2116-5HN32-0DC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=160A overload protection Ir=63A...160A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",707,"ST",1,"LP",1,"3VA21165HN320DC0"]
["3VA2116-6HL32-0KC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU320, LI, In=160A overload protection Ir=63A...160A short-circuit protection Ii=1.5...10 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ",712,"ST",1,"LP",1,"3VA21166HL320KC0"]
["3VA2116-6HN46-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 4-pole, line protection ETU350, LSI, In=160A overload protection Ir=63A...160A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In N conductor protection adjustable (OFF, 50%, 100%) clamp connection",872,"ST",1,"LP",1,"3VA21166HN460AA0"]
["3VA2116-8KQ36-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class L Icu=150kA @ 415V 3-pole, line protection ETU860, LSIG, In=160A overload protection Ir=63A...160A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s clamp connection",1198,"ST",1,"LP",1,"3VA21168KQ360AA0"]
["3VA2125-7JP36-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU550, LSI, In=25A overload protection Ir=10A...25A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% clamp connection",674,"ST",1,"LP",1,"3VA21257JP360AA0"]
["3VA2140-5JQ42-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU560, LSIG, In=40A overload protection Ir=16A...40A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) gr.-fault prot., can be sw. off Ig=0.4...1 x In= tg=0.05-0.8s nut keeper kit",837,"ST",1,"LP",1,"3VA21405JQ420AA0"]
["3VA2140-6KQ36-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU860, LSIG, In=40A overload protection Ir=16A...40A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.4... 1 x In, tg=0.05-0.8s clamp connection",868,"ST",1,"LP",1,"3VA21406KQ360AA0"]
["3VA2140-8JQ32-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class L Icu=150kA @ 415V 3-pole, line protection ETU560, LSIG, In=40A overload protection Ir=16A...40A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.4... 1 x In, tg=0.05-0.8s nut keeper kit",853,"ST",1,"LP",1,"3VA21408JQ320AA0"]
["3VA2163-5HN36-0BA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In clamp connection undervoltage release (UVR) 24V DC",477,"ST",1,"LP",1,"3VA21635HN360BA0"]
["3VA2163-5JP32-0HC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU550, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer nut keeper kit shunt trip (STL) 12-30V DC; 24V AC 50/60Hz 2 auxiliary switches HQ",689,"ST",1,"LP",1,"3VA21635JP320HC0"]
["3VA2163-5KP32-0KH0","circuit breaker 3VA2 IEC frame 160 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU850, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer nut keeper kit shunt trip (STL) 220-250V DC; 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ",831,"ST",1,"LP",1,"3VA21635KP320KH0"]
["3VA2163-6HL36-0DC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU320, LI, In=63A overload protection Ir=25A...63A short-circuit protection Ii=1.5...12 x In clamp connection undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",506,"ST",1,"LP",1,"3VA21636HL360DC0"]
["3VA2163-6JP42-0AA0","circuit breaker 3VA2 IEC frame 160 breaking capacity class H Icu=85kA @ 415V 4-pole, line protection ETU550, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) nut keeper kit",725,"ST",1,"LP",1,"3VA21636JP420AA0"]
["3VA2163-7MN32-0AD0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 3-pole, motor protection ETU350M, LSI, In=63A overload protection Ir=25A...63A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit 3 auxiliary switches HQ",483,"ST",1,"LP",1,"3VA21637MN320AD0"]
["3VA2163-7MS36-0DC0","circuit breaker 3VA2 IEC frame 160 breaking capacity class C Icu=110kA @ 415V 3-pole, starter protection ETU310M, I, In=63A overload protection Ir=25A...63A short-circuit protection Ii=3...15 x In clamp connection undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",435,"ST",1,"LP",1,"3VA21637MS360DC0"]
["3VA2216-5MN32-0AH0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=160A overload protection Ir=63A...160A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit 2 auxiliary switches HQ 1 trip alarm switch HQ",690,"ST",1,"LP",1,"3VA22165MN320AH0"]
["3VA2216-7MN32-0AE0","circuit breaker 3VA2 IEC frame 250 breaking capacity class C Icu=110kA @ 415V 3-pole, motor protection ETU350M, LSI, In=160A overload protection Ir=63A...160A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit 4 auxiliary switches HQ",826,"ST",1,"LP",1,"3VA22167MN320AE0"]
["3VA2220-5MN32-0BC0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, motor protection ETU350M, LSI, In=200A overload protection Ir=80A...200A short-circuit protection Isd=3...15 x Ir, Ii=15 x In nut keeper kit undervoltage release (UVR) 24V DC",849,"ST",1,"LP",1,"3VA22205MN320BC0"]
["3VA2225-5HL42-0AH0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU320, LI, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...10 x In N conductor protection adjustable (OFF, 50%, 100%) nut keeper kit 2 auxiliary switches HQ 1 trip alarm switch HQ",993,"ST",1,"LP",1,"3VA22255HL420AH0"]
["3VA2225-5HN42-0BL0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU350, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In N conductor protection adjustable (OFF, 50%, 100%) nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",1141,"ST",1,"LP",1,"3VA22255HN420BL0"]
["3VA2225-5JP32-0JH0","circuit breaker 3VA2 IEC frame 250 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU550, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",1035,"ST",1,"LP",1,"3VA22255JP320JH0"]
["3VA2225-6HL32-0KL0","circuit breaker 3VA2 IEC frame 250 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU320, LI, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...10 x In nut keeper kit shunt trip (STL) 220-250V DC, 208-277V AC 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",940,"ST",1,"LP",1,"3VA22256HL320KL0"]
["3VA2225-6JQ32-0BC0","circuit breaker 3VA2 IEC frame 250 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU560, LSIG, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ",1280,"ST",1,"LP",1,"3VA22256JQ320BC0"]
["3VA2225-7HL32-0DC0","circuit breaker 3VA2 IEC frame 250 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU320, LI, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...10 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",987,"ST",1,"LP",1,"3VA22257HL320DC0"]
["3VA2225-7KP32-0DA0","circuit breaker 3VA2 IEC frame 250 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU850, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz",1280,"ST",1,"LP",1,"3VA22257KP320DA0"]
["3VA2325-5HN32-0HC0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz 2 auxiliary switches HQ",1107,"ST",1,"LP",1,"3VA23255HN320HC0"]
["3VA2325-6HL32-0BC0","circuit breaker 3VA2 IEC frame 400 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU320, LI, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...12 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ",1182,"ST",1,"LP",1,"3VA23256HL320BC0"]
["3VA2325-6HN32-0AB0","circuit breaker 3VA2 IEC frame 400 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=250A overload protection Ir=100A...250A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit 2 auxiliary switches HP",1182,"ST",1,"LP",1,"3VA23256HN320AB0"]
["3VA2325-7MS32-0BH0","circuit breaker 3VA2 IEC frame 400 breaking capacity class C Icu=110kA @ 415V 3-pole, starter protection ETU310M, I, In=250A without overload protection short-circuit protection Ii=3...15 x In nut keeper kit undervoltage release 24V DC 2 auxiliary switches 1 trip alarm switch",1135,"ST",1,"LP",1,"3VA23257MS320BH0"]
["3VA2340-5HN42-0JL0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 4-pole, line protection ETU350, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In N conductor protection adjustable (OFF, 50%, 100%) nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",1444,"ST",1,"LP",1,"3VA23405HN420JL0"]
["3VA2340-5JQ32-0AJ0","circuit breaker 3VA2 IEC frame 400 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU560, LSIG, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6...10 x In, Ii=1.5 x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit 2 auxiliary switches HP 1 trip alarm switch HP",1391,"ST",1,"LP",1,"3VA23405JQ320AJ0"]
["3VA2340-6HL32-0JL0","circuit breaker 3VA2 IEC frame 400 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU320, LI, In=400A overload protection Ir=160A...400A short-circuit protection Ii=1.5...10 x In nut keeper kit shunt trip (STL) 110-127V DC, AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",1205,"ST",1,"LP",1,"3VA23406HL320JL0"]
["3VA2340-6HN32-0HA0","circuit breaker 3VA2 IEC frame 400 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=1.5...10 x Ir, Ii=10 x In nut keeper kit shunt trip (STL) 12-30V DC, 24V AC 50/60Hz",1187,"ST",1,"LP",1,"3VA23406HN320HA0"]
["3VA2340-7HL32-0DC0","circuit breaker 3VA2 IEC frame 400 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU320, LI, In=400A overload protection Ir=160A...400A short-circuit protection Ii=1.5...10 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",1285,"ST",1,"LP",1,"3VA23407HL320DC0"]
["3VA2340-8KQ42-0AA0","circuit breaker 3VA2 IEC frame 400 breaking capacity class L Icu=150kA @ 415V 4-pole, line protection ETU860, LSIG, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection adjustable (OFF, up to 100%) gr.-fault prot., can be sw. off Ig=0.2...1 x In= tg=0.05-0.8s nut keeper kit",2322,"ST",1,"LP",1,"3VA23408KQ420AA0"]
["3VA2440-6HL32-0DC0","circuit breaker 3VA2 IEC frame 630 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU320, LI, In=400A overload protection Ir=160A...400A short-circuit protection Ii=1.5...12 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",1571,"ST",1,"LP",1,"3VA24406HL320DC0"]
["3VA2440-7HL32-0DC0","circuit breaker 3VA2 IEC frame 630 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU320, LI, In=400A overload protection Ir=160A...400A short-circuit protection Ii=1.5...12 x In nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ",1691,"ST",1,"LP",1,"3VA24407HL320DC0"]
["3VA2440-7JQ32-0BL0","circuit breaker 3VA2 IEC frame 630 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU560, LSIG, In=400A overload protection Ir=160A...400A short-circuit protection Isd=0.6..10x In, Ii=1.5..15x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",2023,"ST",1,"LP",1,"3VA24407JQ320BL0"]
["3VA2450-6JP42-0AA0","circuit breaker 3VA2 IEC frame 630 breaking capacity class H Icu=85kA @ 415V 4-pole, line protection ETU550, LSI, In=500A overload protection Ir=200A...500A short-circuit protection Isd=0.6..10x In, Ii=1.5..14x In N conductor protection adjustable (OFF, up to 100%) nut keeper kit",2033,"ST",1,"LP",1,"3VA24506JP420AA0"]
["3VA2463-5HL32-0AC0","circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=630A overload protection Ir=250A...630A short-circuit protection Ii=1.5...9 x In nut keeper kit 2 auxiliary switches HQ",1319,"ST",1,"LP",1,"3VA24635HL320AC0"]
["3VA2463-5KP32-0AD0","circuit breaker 3VA2 IEC frame 630 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU850, LSI, In=630A overload protection Ir=250A...630A short-circuit protection Isd=0.6..9 x In, Ii=1.5..9 x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit 3 auxiliary switches HQ",1631,"ST",1,"LP",1,"3VA24635KP320AD0"]
["3VA2463-6HN32-0CH0","circuit breaker 3VA2 IEC frame 630 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=630A overload protection Ir=250A...630A short-circuit protection Isd=1.5...9 x Ir, Ii=9 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",1657,"ST",1,"LP",1,"3VA24636HN320CH0"]
["3VA2463-6JP32-0BH0","circuit breaker 3VA2 IEC frame 630 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU550, LSI, In=630A overload protection Ir=250A...630A short-circuit protection Isd=0.6..9 x In, Ii=1.5..9 x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ",1738,"ST",1,"LP",1,"3VA24636JP320BH0"]
["3VA2463-7HN32-0AJ0","circuit breaker 3VA2 IEC frame 630 breaking capacity class C Icu=110kA @ 415V 3-pole, line protection ETU350, LSI, In=630A overload protection Ir=250A...630A short-circuit protection Isd=1.5...9 x Ir, Ii=9 x In nut keeper kit 2 auxiliary switches HP 1 trip alarm switch HP",1726,"ST",1,"LP",1,"3VA24637HN320AJ0"]
["3VA2510-5HL32-0CL0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU320, LI, In=1000A overload protection Ir=400A...1000A short-circuit protection Ii=1.5...10 x In nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ 1 electrical alarm switch",2625,"ST",1,"LP",1,"3VA25105HL320CL0"]
["3VA2510-5KQ32-0DH0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU860, LSIG, In=1000A overload protection Ir=400A...1000A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection optionally with external current transformer, up to 160% gr.-fault prot., can be sw. off Ig=0.2...1 x In, tg=0.05-0.8s nut keeper kit undervoltage release (UVR) 208-230V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ.",2984,"ST",1,"LP",1,"3VA25105KQ320DH0"]
["3VA2563-6HM42-0AA0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class H Icu=85kA @ 415V 4-pole, line protection ETU330, LIG, In=630A overload protection Ir=250A...630A short-circuit protection Ii=1.5...12 x In N conductor protection adjustable (OFF, 50%, 100%) ground-fault protection Ig=0.2...1 x In= tg=0.1/0.3s nut keeper kit",1973,"ST",1,"LP",1,"3VA25636HM420AA0"]
["3VA2580-5HN32-0BH0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU350, LSI, In=800A overload protection Ir=320A...800A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ",1960,"ST",1,"LP",1,"3VA25805HN320BH0"]
["3VA2580-5JP32-0CH0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class M Icu=55kA @ 415V 3-pole, line protection ETU550, LSI, In=800A overload protection Ir=320A...800A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% nut keeper kit undervoltage release (UVR) 120-127V AC 50/60Hz 2 auxiliary switches HQ 1 trip alarm switch HQ",2003,"ST",1,"LP",1,"3VA25805JP320CH0"]
["3VA2580-6HN32-0BH0","circuit breaker 3VA2 IEC frame 1000 breaking capacity class H Icu=85kA @ 415V 3-pole, line protection ETU350, LSI, In=800A overload protection Ir=320A...800A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In nut keeper kit undervoltage release (UVR) 24V DC 2 auxiliary switches HQ 1 trip alarm switch HQ",2241,"ST",1,"LP",1,"3VA25806HN320BH0"]
["3VA4112-5ED14-3AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class M 35kA @ 277 V 1-pole, line protection TM210, FTFM, In=125A overload protection Ir=125A fixed short circuit protection Ii=10 x In",262,"ST",1,"LP",36,"3VA41125ED143AA0"]
["3VA4130-5ED24-1AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class M 35kA @ 480 V 2-pole, line protection TM210,  FTFM, In=30A overload protection Ir=30A fixed short-circuit protection Ii=10 x In UL489 SB (naval), 50 deg. cel. clamp connection",237,"ST",1,"LP",1,"3VA41305ED241AA0"]
["3VA4135-6ED24-0AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class H 65kA @ 480 V 2-pole, line protection TM210,  FTFM, In=35A overload protection Ir=35A fixed short-circuit protection Ii=10 x In clamp connection",246,"ST",1,"LP",1,"3VA41356ED240AA0"]
["3VA4150-5ED24-1AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class M 35kA @ 480 V 2-pole, line protection TM210,  FTFM, In=50A overload protection Ir=50A fixed short-circuit protection Ii=10 x In UL489 SB (naval), 50 deg. cel. clamp connection",237,"ST",1,"LP",1,"3VA41505ED241AA0"]
["3VA4190-6ED54-0AA0","circuit breaker 3VA4 UL frame 125 breaking capacity class H 65kA @ 277 V 1-pole, line protection TM210,  FTFM, In=90A overload protection Ir=90A fixed short-circuit protection Ii=10 x In clamp connection",240,"ST",1,"LP",1,"3VA41906ED540AA0"]
["3VA5110-6EF41-0BC0","circuit breaker 3VA5 UL frame 125 breaking capacity class H 65kA @ 480V 4-pole, line protection TM240, ATAM, In=100A overload protection Ir=80A...100A short-circuit protection Ii=5...10 x In N conductor unprotected without connection circuit breaker 3VA5 UL frame 125 breaking capacity class H 65kA @ 480V 4-pole, line protection TM240, ATAM, In=100A overload protection Ir=80A...100A short-circuit",626,"ST",1,"LP",1,"3VA51106EF410BC0"]
["3VA5112-4ED21-0AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class S 25kA @ 480V 2-pole, line protection TM210, FTFM, In=125A overload protection Ir=125A fixed short-circuit protection Ii=10 x In without connection",428,"ST",1,"LP",1,"3VA51124ED210AA0"]
["3VA5135-6ED31-0AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class H 65kA @ 480V 3-pole, line protection TM210, FTFM, In=35A overload protection Ir=35A fixed short-circuit protection Ii=10 x In without connection",264,"ST",1,"LP",1,"3VA51356ED310AA0"]
["3VA5150-6ED31-0AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class H 65kA @ 480V 3-pole, line protection TM210, FTFM, In=50A overload protection Ir=50A fixed short-circuit protection Ii=10 x In without connection",264,"ST",1,"LP",1,"3VA51506ED310AA0"]
["3VA5160-5ED21-0AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class M 35kA @ 480 V 2-pole, line protection TM210, FTFM, In=60A overload protection Ir=60A fixed short-circuit protection Ii=10 x In without connection",224,"ST",1,"LP",1,"3VA51605ED210AA0"]
["3VA5180-5ED21-0AA0","circuit breaker 3VA5 UL frame 125 breaking capacity class M 35kA @ 480 V 2-pole, line protection TM210, FTFM, In=80A overload protection Ir=80A fixed short-circuit protection Ii=10 x In without connection",245,"ST",1,"LP",1,"3VA51805ED210AA0"]
["3VA5211-5ED31-0AA0","circuit breaker 3VA5 UL frame 250 breaking capacity class M 35kA @ 480 V 3-pole, line protection TM210, FTFM, In=110A overload protection Ir=110A fixed short-circuit protection Ii=10 x In without connection",652,"ST",1,"LP",1,"3VA52115ED310AA0"]
["3VA5215-5EC41-0AA0","circuit breaker 3VA5 UL frame 250 breaking capacity class M 35kA @ 480 V 4-pole, line protection TM230, FTAM, In=150A overload protection Ir=150A fixed short-circuit protection Ii=5...10 x In N conductor unprotected without connection",1003,"ST",1,"LP",1,"3VA52155EC410AA0"]
["3VA5220-0MH31-0BA0","circuit breaker 3VA5 UL frame 250 3-pole, starter protection TM120M, AM, In=200A without overload protection short-circuit protection Ii=6...12 x In without connection",1025,"ST",1,"LP",1,"3VA52200MH310BA0"]
["3VA5225-7GC41-0AA0","circuit breaker 3VA5 UL frame 250 breaking capacity class C 100kA @ 480V 4-pole, line protection TM230, FTAM, In=250A overload protection Ir=250A fixed short-circuit protection Ii=5...10 x In N conductor protection 100% without connection",1441,"ST",1,"LP",1,"3VA52257GC410AA0"]
["3VA5280-6ED31-0AA0","circuit breaker 3VA5 UL frame 250 breaking capacity class H 65kA @ 480V 3-pole, line protection TM210, FTFM, In=80A overload protection Ir=80A fixed short-circuit protection Ii=10 x In without connection",624,"ST",1,"LP",1,"3VA52806ED310AA0"]
["3VA5322-6EC61-0AA0","CIRCUIT BREAKER 3VA5 UL Frame 400 BREAKING CAPACITY CLASS  H 65kA @ 480 V 2POLE, LINE PROTECTION TM230,  FTAM, In=225A WITHOUT OVERLOAD PROTECTION IR=225A FIXED SHORT CIRCUIT PROTECTION Ii=5...10 x In W/O CONNECTION",1047,"ST",1,"LP",1,"3VA53226EC610AA0"]
["3VA5445-6EF41-0AA0","CIRCUIT BREAKER 3VA5 UL Frame 600 BREAKING CAPACITY CLASS  H 65kA @ 480 V 4POLE, LINE PROTECTION TM240,  ATAM, In=450A WITHOUT OVERLOAD PROTECTION IR=315A ...450A SHORT CIRCUIT PROTECTION Ii=5...10 x In NEUTRAL UNPROTECTED W/O CONNECTION",2473,"ST",1,"LP",1,"3VA54456EF410AA0"]
["3VA5445-7EF31-0AA0","CIRCUIT BREAKER 3VA5 UL FRAME 600 BREAKING CAPACITY CLASS  C 100kA @ 480 V 3POLE, LINE PROTECTION TM240,  ATAM, In=450A OVERLOAD PROTECTION IR=315A ...450A SHORT CIRCUIT PROTECTION II=5...10 X IN W/O CONNECTION",2064,"ST",1,"LP",1,"3VA54457EF310AA0"]
["3VA5570-7EC36-0AA0","circuit breaker 3VA5 UL frame 800 breaking capacity class  C 100kA @ 480 V 3-pole, line protection TM230,  FTAM, In=700A overload protection Ir=700A fixed short circuit protection Ii=5...10 x In",2851,"ST",1,"LP",1,"3VA55707EC360AA0"]
["3VA6110-5JT31-0AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class M 35kA @ 480V 3-pole, line protection ETU556, LSI, In=100A overload protection Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% ground-fault alarm message via EFB300 or COM without connection",1069,"ST",1,"LP",1,"3VA61105JT310AA0"]
["3VA6110-8KP31-2AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class L 150kA @ 480V 3-pole, line protection ETU850, LSI, In=100A overload protection, 100% rated Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% without connection",1656,"ST",1,"LP",1,"3VA61108KP312AA0"]
["3VA6115-6JP41-0AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class H 65kA @ 480V 4-pole, line protection ETU550, LSI, In=150A overload protection Ir=60A...150A short-circuit protection Isd=0.6..10x In, Ii=1.5..10x In N conductor protection adjustable (OFF, up to 100%) without connection",1738,"ST",1,"LP",1,"3VA61156JP410AA0"]
["3VA6115-8HM41-0AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class L 150kA @ 480V 4-pole, line protection ETU330, LIG, In=150A overload protection Ir=60A...150A short-circuit protection Ii=1.5...10 x In N conductor protection adjustable (OFF, 100%) ground-fault protection Ig=0.2...1 x In= tg=0.1/0.3s without connection",1775,"ST",1,"LP",1,"3VA61158HM410AA0"]
["3VA6140-6HN31-2AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class H 65kA @ 480V 3-pole, line protection ETU350, LSI, In=40A overload protection, 100% rated Ir=16A...40A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In without connection",686,"ST",1,"LP",1,"3VA61406HN312AA0"]
["3VA6160-0KT31-0AA0","circuit breaker 3VA6 UL frame 150 breaking capacity class  E 200 kA @ 480 V 3-pole, line protection ETU856,  LSI, In=60A overload protection Ir=24A ...60A short circuit protection Isd=1,5..10x In, Ii=1,5..12x In neutral protection optional with ext. CT;up to160% ground fault alarm alarm via EFB300 or COM w/o connection",1686,"ST",1,"LP",1,"3VA61600KT310AA0"]
["3VA6210-6KM41-0AA0","circuit breaker 3VA6 UL frame 250 breaking capacity class H 65kA @ 480V 4-pole, line protection ETU830, LIG, In=100A overload protection Ir=40A...100A short-circuit protection Ii=1.5...12 x In ground-fault protection Ig=0.2...1 x In, tg=0.05-0.8s without connection",2539,"ST",1,"LP",1,"3VA62106KM410AA0"]
["3VA6210-7KP41-2AA0","circuit breaker 3VA6 UL frame 250 breaking capacity class C 100kA @ 480V 4-pole, line protection ETU850, LSI, In=100A overload protection, 100% rated Ir=40A...100A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) without connection",2755,"ST",1,"LP",1,"3VA62107KP412AA0"]
["3VA6225-5KM31-0AA0","circuit breaker 3VA6 UL frame 250 breaking capacity class M 35kA @ 480V 3-pole, line protection ETU830, LIG, In=250A overload protection Ir=100A...250A short-circuit protection Ii=1.5...10 x In ground-fault protection Ig=0.2...1 x In, tg=0.05-0.8s without connection",2012,"ST",1,"LP",1,"3VA62255KM310AA0"]
["3VA6325-0HL31-0AA0","circuit breaker 3VA6 UL frame 400 breaking capacity class  E 200 kA @ 480 V 3-pole, line protection ETU320,  LI, In=250A overload protection Ir=100A ... 250A short circuit protection Ii=1,5...12 x In w/o connection",2131,"ST",1,"LP",1,"3VA63250HL310AA0"]
["3VA6325-5KQ41-0AA0","circuit breaker 3VA6 UL frame 400 breaking capacity class M 35kA @ 480V 4-pole, line protection ETU860, LSIG, In=250A overload protection Ir=100A...250A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection adjustable (OFF, up to 160%) ground-fault protection Ig=0.2...1 x In= tg=0.05-0.8s without connection",2814,"ST",1,"LP",1,"3VA63255KQ410AA0"]
["3VA6340-0HN41-0AA0","circuit breaker 3VA6 UL frame 400 breaking capacity class  E 200 kA @ 480 V 4-pole, line protection ETU350,  LSI, In=400A overload protection Ir=160A ... 400A short circuit protection Isd=1,5... 10 x Ir, Ii=12 x In neutral protection adjustable(OFF; 50%; 100%) w/o connection",3000,"ST",1,"LP",1,"3VA63400HN410AA0"]
["3VA6340-8HM31-0AA0","circuit breaker 3VA6 UL frame 400 breaking capacity class L 150kA @ 480V 3-pole, line protection ETU330, LIG, In=400A overload protection Ir=160A...400A short-circuit protection Ii=1.5...10 x In ground-fault protection Ig=0.2...1 x In, tg=0.1/0.3s without connection",2272,"ST",1,"LP",1,"3VA63408HM310AA0"]
["3VA6440-6HN41-0AA0","circuit breaker 3VA6 UL frame 600 breaking capacity class H 65kA @ 480V 4-pole, line protection ETU350, LSI, In=400A overload protection Ir=160A...400A short-circuit protection Isd=1.5...10 x Ir, Ii=12 x In N conductor protection adjustable (OFF, 50%, 100%) without connection",3029,"ST",1,"LP",1,"3VA64406HN410AA0"]
["3VA6440-8JP31-2AA0","circuit breaker 3VA6 UL frame 600 breaking capacity class L 150kA @ 480V 3-pole, line protection ETU550, LSI, In=400A overload protection, 100% rated Ir=160A...400A short-circuit protection Isd=0.6..10x In, Ii=1.5..12x In N conductor protection optionally with external current transformer, up to 160% without connection",3653,"ST",1,"LP",1,"3VA64408JP312AA0"]
["3VA6460-8KQ41-0AA0","circuit breaker 3VA6 UL frame 600 breaking capacity class L 150kA @ 480V 4-pole, line protection ETU860, LSIG, In=600A overload protection Ir=240A...600A short-circuit protection Isd=0.6..9x In, Ii=1.5..9x In N conductor protection adjustable (OFF, up to 100%) ground-fault protection Ig=0.2...1 x In= tg=0.05-0.8s without connection",4625,"ST",1,"LP",1,"3VA64608KQ410AA0"]
["3VA6560-6HL46-0AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  H 65kA @ 480 V 4-pole, line protection ETU320,  LI, In=600A overload protection Ir=240A ...600A short circuit protection Ii=1,5...12 x In",3430,"ST",1,"LP",1,"3VA65606HL460AA0"]
["3VA6560-7HM46-2AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  C 100kA @ 480 V 4-pole, line protection ETU330, LIG, In=600A overload protection, 100% rated Ir=240A...600A short circuit protection Ii=1,5...12 x In",4336,"ST",1,"LP",1,"3VA65607HM462AA0"]
["3VA6580-5HL46-0AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  M 35kA @ 480 V 4-pole, line protection ETU320,  LI, In=800A overload protection Ir=320A ...800A short circuit protection Ii=1,5...10 x In",4165,"ST",1,"LP",1,"3VA65805HL460AA0"]
["3VA6580-7JP32-0AA0","circuit breaker 3VA6 UL frame 800 breaking capacity class  C 100kA @ 480 V 3-pole, line protection ETU550,  LSI, In=800A overload protection Ir=320A ...800A short circuit protection",4002,"ST",1,"LP",1,"3VA65807JP320AA0"]
["3VA6610-5HL36-0AA0","circuit breaker 3VA6 UL frame 1000 breaking capacity class  M 35kA @ 480 V 3-pole, line protection ETU320,  LI, In=1000A overload protection Ir=400A ...1000A short circuit protection Ii=1,5...12 x In",4173,"ST",1,"LP",1,"3VA66105HL360AA0"]
["3VA9111-0QF10","rear connection stud round short 1 unit accessory for: 3VA1 100/160",10.299999999999999,"ST",1,"LP",1,"3VA91110QF10"]
["3VA9113-0JB11","wire connector 3 units accessory for: 3VA1 100/160",15.799999999999999,"ST",1,"LP",1,"3VA91130JB11"]
["3VA9137-0PK17","side wall mounted rot. operator emergency-off IEC IP65 24V DC lighting kit accessory for: 3VA5 125",183,"ST",1,"LP",1,"3VA91370PK17"]
["3VA9157-0KP81","autotrip plunger accessory for: plug-in unit 3VA1 100/160",27.8,"ST",1,"LP",1,"3VA91570KP81"]
["3VA9213-0KB01","terminal cover plug-in and draw-out technology accessory for: circuit breaker, 3-pole 3VA1 250",34,"ST",1,"LP",1,"3VA92130KB01"]
["3VA9253-0JB12","wire connector 3 units accessory for: 3VA1 250",22.6,"ST",1,"LP",1,"3VA92530JB12"]
["3VA9264-0QD00","bus connector extended edgewise 4 units accessory for: 3VA2 100/160/250",33.700000000000003,"ST",1,"LP",1,"3VA92640QD00"]
["3VA9277-0FK21","door mounted rotary operator standard IEC IP65 with door interlock accessory for: 3VA6 150/250 3VA5 250",99.5,"ST",1,"LP",1,"3VA92770FK21"]
["3VA9447-0FK33","Door mounted rotary operator standard NEMA Type 1, 3R, 12, 4/4X with door interlocking illumination kits 24 V DC and door-open position accessory for 3VA5/6 400/600",211,"ST",1,"LP",1,"3VA94470FK33"]
["3VA9477-0GA80","RETAINING BRACKET ACCESSORY FOR 3VA5 250/400/600 and 3VA6 150/250/400/600",31.6,"ST",1,"LP",1,"3VA94770GA80"]
["3VA9603-0SS10","Mounting screw kit consists of 4 screws and nuts, metric thread accessory for: plug-in unit 3VA9603-0KP00",25.3,"ST",1,"LP",1,"3VA96030SS10"]
["3VA9673-0JJ43","wire connector for 4 cables; 3 pcs. accessory for: 3VA55/3VA65/3VA66",248,"ST",1,"LP",1,"3VA96730JJ43"]
["3VA9980-0VC20","Bowden cable (1.0m/39.370\") accessory for: Bowden cable interlock module",49.6,"ST",1,"LP",1,"3VA99800VC20"]
["3VL1110-2KE30-0AA0","circuit breaker VL150X UL, type CG (cat no. HCS3S100) non-interchangeable frame, with circuit breaker approval acc. to UL 489 high breaking capacity 3-pole, NEMA rating 65kA/480V (molded case switch) trip unit, magnetic TA=40Β°C In=<100A rated current II=1800A short-circuit protection without connection accessories without auxiliary release without auxiliary/alarm switch",519,"ST",1,"LP",1,"3VL11102KE300AA0"]
["3VL1703-2DD33-0AA0","circuit breaker VL160X H high breaking capacity Icu=70kA, 415V AC 3-pole, line protection Trip Unit TM, LI In=32A, rated current Ir=32A, overload protection II=300A, short-circuit prot. without auxiliary release without auxiliary/alarm switch",510,"ST",1,"LP",1,"3VL17032DD330AA0"]
["3VL1708-1DD33-0AA0","circuit breaker VL160X N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection   Trip Unit TM, LI In=80A, rated current Ir=63...80A, overload prot. II=1000A, short-circuit prot. without auxiliary release without auxiliary/alarm switch",474,"ST",1,"LP",1,"3VL17081DD330AA0"]
["3VL1710-2DD36-0AA0","circuit breaker VL160X H high breaking capacity Icu=70kA, 415V AC 3-pole, line protection Trip Unit TM, LI In=100A, rated current Ir=100A, overload protection II=1000A, short-circuit prot. with screw terminals without auxiliary release without auxiliary/alarm switch",607,"ST",1,"LP",1,"3VL17102DD360AA0"]
["3VL1725-1EH46-0AA0","circuit breaker VL160X N standard breaking capacity Icu=55kA, 415V AC 4-pole, line protection   Trip Unit TM, LI In=25A, rated current Ir=25A, overload protection II=300A, short-circuit prot. N unprotected with screw terminals without auxiliary release without auxiliary/alarm switch",500,"ST",1,"LP",1,"3VL17251EH460AA0"]
["3VL1796-1DA33-2SD1","circuit breaker VL160X N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection   Trip Unit TM, LI In=16A, rated current Ir=16A, overload protection II=300A, short-circuit prot. Undervoltage release 220...250 V DC Auxiliary/alarm switch mounting kit 2 AUX (1 NO+1 NC)+1 AS (1 NO)",732,"ST",1,"LP",1,"3VL17961DA332SD1"]
["3VL2706-1DK33-0AB1","circuit breaker VL160N standard breaking capacity Icu=55kA, 415V AC 3-pole, starter combination   Trip Unit magnetic In=63A, rated current II=450...900A, short-circuit protection without auxiliary release Auxiliary switch mounting kit 2 AUX (1 NO + 1 NC)",508,"ST",1,"LP",1,"3VL27061DK330AB1"]
["3VL2706-2DC36-2SD1","circuit breaker VL160H high breaking capacity Icu=70kA, 415V AC 3-pole, line protection Trip Unit TM, LI In=63A, rated current IR=50...63A, overload protection, II=300...600A, short-circuit protection with screw terminals Undervoltage release 220...250 V DC Auxiliary/alarm switch mounting kit 2 AUX (1 NO+1 NC)+1 AS (1 NO)",859,"ST",1,"LP",1,"3VL27062DC362SD1"]
["3VL2706-2MH36-0AA0","circuit breaker VL160H high breaking capacity Icu=70kA, 415V AC 3-pole, line protection Electronic Trip Unit ETU22, LSIG 3 phases/4 lines with connecting cable In=63A, rated current IR=25...63A, overload protection, ISD=1.5 to 10xIR, II=11xIN with screw terminals without auxiliary release ETU communication-capable without auxiliary/alarm switch",1327,"ST",1,"LP",1,"3VL27062MH360AA0"]
["3VL2706-3MB33-0AA0","circuit breaker VL160L very high breaking capacity Icu=100kA, 415V AC 3-pole, line protection Electronic Trip Unit ETU10, LI In=63A, rated current IR=25...63A, overload protection, II=1.25 to 11xIN, short-circuit protection without auxiliary release ETU communication-capable without auxiliary/alarm switch",1355,"ST",1,"LP",1,"3VL27063MB330AA0"]
["3VL2710-1EE43-0AB1","circuit breaker VL160N standard breaking capacity Icu=55kA, 415V AC 4-pole, non-auto. air circ. br.   Trip Unit magnetic In=100A, rated current II=2500A, short-circuit protection without auxiliary release Auxiliary switch mounting kit 2 AUX (1 NO + 1 NC)",643,"ST",1,"LP",1,"3VL27101EE430AB1"]
["3VL2710-1TA46-0AA0","circuit breaker VL160N standard breaking capacity Icu=55kA, 415V AC 4-pole, line protection Electronic Trip Unit ETU10, LIN In=100A, rated current IR=40...100A, overload protection, II=1.25 to 11xIN, short-circuit protection N protected with screw terminals without auxiliary release without auxiliary/alarm switch",1176,"ST",1,"LP",1,"3VL27101TA460AA0"]
["3VL2710-2NH46-0AA0","circuit breaker VL160H high breaking capacity Icu=70kA, 415V AC 4-pole, line protection Electronic Trip Unit ETU22, LSIG In=100A, rated current IR=40...100A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection N protected with screw terminals without auxiliary release ETU communication-capable without auxiliary/alarm switch",1787,"ST",1,"LP",1,"3VL27102NH460AA0"]
["3VL2712-1DC33-2JA0","circuit breaker VL160N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection Trip Unit TM, LI In=125A, rated current IR=100...125A, overload protection, II=625...1250A, short-circuit protection Undervoltage release 380...415 V AC without auxiliary/alarm switch",1139,"ST",1,"LP",1,"3VL27121DC332JA0"]
["3VL2712-1EJ46-0AB1","circuit breaker VL160N standard breaking capacity Icu=55kA, 415V AC 4-pole, line protection Trip Unit TM, LI In=125A, rated current IR=100...125A, overload protection, II=625...1250A, short-circuit protection N unprotected with screw terminals without auxiliary release Auxiliary switch mounting kit 2 AUX (1 NO + 1 NC)",1258,"ST",1,"LP",1,"3VL27121EJ460AB1"]
["3VL2716-1MH36-0AA0","circuit breaker VL160N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection Electronic Trip Unit ETU22, LSIG 3 phases/4 lines with connecting cable In=160A, rated current IR=64...160A, overload protection, ISD=1.5 to 10xIR, II=11xIN with screw terminals without auxiliary release ETU communication-capable without auxiliary/alarm switch",1929,"ST",1,"LP",1,"3VL27161MH360AA0"]
["3VL2716-2DC33-2SD1","circuit breaker VL160H high breaking capacity Icu=70kA, 415V AC 3-pole, line protection Trip Unit TM, LI In=160A, rated current IR=125...160A, overload protection, II=800...1600A, short-circuit protection Undervoltage release 220...250 V DC Auxiliary/alarm switch mounting kit 2 AUX (1 NO+1 NC)+1 AS (1 NO)",1487,"ST",1,"LP",1,"3VL27162DC332SD1"]
["3VL2716-3MP36-0AA0","circuit breaker VL160L very high breaking capacity Icu=100kA, 415V AC 3-pole, motor/generator prot. Electronic Trip Unit ETU10M, LI In=160A, rated current IR=64...160A, overload protection, II=1.25 to 11xIN, short-circuit protection with screw terminals without auxiliary release ETU communication-capable without auxiliary/alarm switch",1712,"ST",1,"LP",1,"3VL27163MP360AA0"]
["3VL3110-2PD30-0AA0","circuit breaker VL250 UL; type FG (cat no. HFX3W100) non-interchangeable frame, with circuit breaker approval acc. to UL 489 high breaking capacity 3-pole, NEMA rating 65kA/480V, (molded case circuit breaker) Electronic Trip Unit ETU, LIG TA=40Β°C 3 phases/4 lines In=100A, rated current II=1.25 to 11xIN, short-circuit protection IR=40-100A Electronic Trip Unit for line protection without connection accessories without auxiliary release without auxiliary/alarm switch",1769,"ST",1,"LP",1,"3VL31102PD300AA0"]
["3VL3125-3VJ30-0AA0","circuit breaker VL250 UL type FG (cat no. LFX3K250) non-interchangeable frame, with circuit breaker approval acc. to UL 489 very high breaking capacity 3-pole; NEMA rating 100kA/480V and 25kA/600V (molded case circuit breaker) Electronic Trip Unit LCD ETU, LSIG-G with alarm TA=40Β°C 3 phases/4 lines In=250A, rated current ISD=1.25-10xIR, II=11X in short-circuit protection IR=70-250A Electronic Trip Unit for line protection without auxiliary release without auxiliary/alarm switch",4327,"ST",1,"LP",1,"3VL31253VJ300AA0"]
["3VL3720-1MG36-0AA0","circuit breaker VL250N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection Electronic Trip Unit ETU22, LSIG 3 phases/3 lines In=200A, rated current IR=80...200A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection without auxiliary release ETU communication-capable without auxiliary/alarm switch",2446,"ST",1,"LP",1,"3VL37201MG360AA0"]
["3VL3720-2DC36-2RD1","circuit breaker VL250H high breaking capacity Icu=70kA, 415V AC 3-pole, line protection Trip Unit TM, LI In=200A, rated current IR=160...200A, overload protection, II=1000...2000A, short-circuit protection Undervoltage release 110...127 V DC Auxiliary/alarm switch mounting kit 2 AUX (1 NO+1 NC)+1 AS (1 NO)",1741,"ST",1,"LP",1,"3VL37202DC362RD1"]
["3VL3720-2UP36-0AA0","circuit breaker VL250H high breaking capacity Icu=70kA, 415V AC 3-pole, motor/generator prot. Electronic Trip Unit LCD ETU40M, LI In=200A, rated current IR=80...200A, overload protection, II=1.25 to 11xIN, short-circuit protection without auxiliary release without auxiliary/alarm switch",3320,"ST",1,"LP",1,"3VL37202UP360AA0"]
["3VL3725-1EJ46-0AA0","circuit breaker VL250N standard breaking capacity Icu=55kA, 415V AC 4-pole, line protection Trip Unit TM, LI In=250A, rated current IR=200...250A, overload protection, II=1200...2500A, short-circuit protection N unprotected without auxiliary release without auxiliary/alarm switch",1853,"ST",1,"LP",1,"3VL37251EJ460AA0"]
["3VL3725-1LE36-0AA0","circuit breaker VL250N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection Trip Unit ETU20, LSI In=250A, rated current IR=100...250A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection without auxiliary release shipbuilding certificate for LRS, DNV and gL without auxiliary/alarm switch",2145,"ST",1,"LP",1,"3VL37251LE360AA0"]
["3VL3725-2NF43-0AA0","circuit breaker VL250H high breaking capacity Icu=70kA, 415V AC 4-pole, line protection Electronic Trip Unit ETU20, LSI In=250A, rated current IR=100...250A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection N protected without auxiliary release with box terminal ETU communication-capable without auxiliary/alarm switch",2972,"ST",1,"LP",1,"3VL37252NF430AA0"]
["3VL3725-2UP36-0AA0","circuit breaker VL250H high breaking capacity Icu=70kA, 415V AC 3-pole, motor/generator prot. Electronic Trip Unit LCD ETU40M, LI In=250A, rated current IR=100...250A, overload protection, II=1.25 to 11xIN, short-circuit protection without auxiliary release without auxiliary/alarm switch",3320,"ST",1,"LP",1,"3VL37252UP360AA0"]
["3VL4140-3PE30-0AA0","circuit breaker VL400 UL; type JG (cat no. LJX3T400) non-interchangeable frame, with circuit breaker approval acc. to UL 489 very high breaking capacity 3-pole, NEMA rating 100kA/480V, (molded case circuit breaker) Electronic Trip Unit ETU, LSI TA=40Β°C In=400A, rated current ISD=1.5 to 10xIR, II=11 xIn short-circuit protection IR=200-400A ETU for line protection without connection accessories without auxiliary release without auxiliary/alarm switch",3828,"ST",1,"LP",1,"3VL41403PE300AA0"]
["3VL4731-1EC46-0AA0","circuit breaker VL400N standard breaking capacity Icu=55kA, 415V AC 4-pole, line protection Trip Unit TM, LI In=315A, rated current IR=250...315A, overload protection, II=1575...3150A, short-circuit protection N protected without auxiliary release without auxiliary/alarm switch",2521,"ST",1,"LP",1,"3VL47311EC460AA0"]
["3VL4731-2LB36-0AA0","circuit breaker VL400H high breaking capacity Icu=70kA, 415V AC 3-pole, line protection Electronic Trip Unit ETU10, LI In=315A, rated current IR=128...315A, overload protection, II=1.25 to 11xIN, short-circuit protection shipbuilding certificate for LRS, DNV and gL without auxiliary release without auxiliary/alarm switch",3085,"ST",1,"LP",1,"3VL47312LB360AA0"]
["3VL4731-3TF46-0AD1","circuit breaker VL400L very high breaking capacity Icu=100kA, 415V AC 4-pole, line protection Electronic Trip Unit ETU20, LSI In=315A, rated current IR=128...315A, overload protection, ISD=1.5 to 10xIR, II=11xIN short-circuit protection N protected without auxiliary release Auxiliary/alarm switch mounting kit 2 AUX (1 NO+1 NC)+1 AS (1 NO)",4977,"ST",1,"LP",1,"3VL47313TF460AD1"]
["3VL4740-2TB46-0AA0","circuit breaker VL400H high breaking capacity Icu=70kA, 415V AC 4-pole, line protection trip unit ETU10, LI In=400A, rated current IR=160...400A, overload protection, II=1.25 to 11xIN, short-circuit protection without auxiliary release without auxiliary/alarm switch",3584,"ST",1,"LP",1,"3VL47402TB460AA0"]
["3VL4860-2PH30-0AA0","circuit breaker VL400X UL; type LG (cat no. HLK3V600) non-interchangeable frame, with circuit breaker approval acc. to UL 489 high breaking capacity 3-pole, NEMA rating 65kA/480V and 18kA/600V (molded case circuit breaker) trip unit ETU, LSIG TA=40Β°C 3 phases/4 lines In=600A, rated current ISD=1.5 to 9xIR, II=10xIN short-circuit protection IR=200-600A ETU for line protection without connection accessories without auxiliary release without auxiliary/alarm switch",5107,"ST",1,"LP",1,"3VL48602PH300AA0"]
["3VL5740-3DC36-0AA0","circuit breaker VL630L very high breaking capacity Icu=100kA, 415V AC 3-pole, line protection trip unit TM, LI In=400A, rated current IR=315...400A, overload protection, II=2000...4000A, short-circuit protection without auxiliary release without auxiliary/alarm switch",3753,"ST",1,"LP",1,"3VL57403DC360AA0"]
["3VL5763-1SF36-0AA0","circuit breaker VL630N standard breaking capacity Icu=55kA, 415V AC 3-pole, line protection trip unit ETU12, LIG 3 phases/4 lines In=630A, rated current IR=252...630A, overload protection, II=1.25 to 10xIN, short-circuit protection without auxiliary release without auxiliary/alarm switch",4524,"ST",1,"LP",1,"3VL57631SF360AA0"]
["3VL6180-1KN30-0AA0","circuit breaker VL800 UL; type MG (cat no. NMX3B800) non-interchangeable frame, with circuit breaker approval acc. to UL 489 standard breaking capacity 3-pole, NEMA rating 35kA/480V, (molded case circuit breaker) trip unit TM, LI TA=40Β°C In=< 800A, rated current II=3250...6500A short-circuit protection IR=800A ETU for line protection without connection accessories without auxiliary release without auxiliary/alarm switch",3640,"ST",1,"LP",1,"3VL61801KN300AA0"]
["3VL6780-1NN46-0AA0","circuit breaker VL800N standard breaking capacity Icu=55kA, 415V AC 4-pole, line protection trip unit ETU12, LIG In=800A, rated current IR=320...800A, overload protection, II=1.25 to 8 xIN, short-circuit protection N protected without auxiliary release ETU communication-capable without auxiliary/alarm switch",6847,"ST",1,"LP",1,"3VL67801NN460AA0"]
["3VL7112-3VJ30-0AA0","circuit breaker VL1200 UL type NG (cat no. LNX3K120) non-interchangeable frame, with circuit breaker approval acc. to UL 489 very high breaking capacity 3-pole; NEMA rating 100kA/480V and 65kA/600V (molded case circuit breaker) trip unit LCD ETU, LSIG-G with alarm TA=40Β°C 3 phases/4 lines In=1200A, rated current ISD=1.25-10xIR, II=10xIN short-circuit protection IR=400-1200A overcurrent rel. for line protection without auxiliary release without auxiliary/alarm switch",10534,"ST",1,"LP",1,"3VL71123VJ300AA0"]
["3VL7710-3LE36-0AA0","circuit breaker VL1250L very high breaking capacity Icu=100kA, 415V AC 3-pole, line protection trip unit ETU20, LSI In=1000A, rated current IR=400...1000A, overload protection, ISD=1.5 to 10xIR, II=11 xIN short-circuit protection shipbuilding certificate for LRS, DNV and gL without auxiliary release without auxiliary/alarm switch",8493,"ST",1,"LP",1,"3VL77103LE360AA0"]
["3VL7712-1NA46-0AA0","circuit breaker VL1250N standard breaking capacity Icu=55kA, 415V AC 4-pole, line protection trip unit ETU10, LIN In=1250A, rated current IR=500...1250A, overload protection, II=1.25 to 10xIN, short-circuit protection N protected without auxiliary release ETU communication-capable without auxiliary/alarm switch",9349,"ST",1,"LP",1,"3VL77121NA460AA0"]
["3VL7712-3ML36-0AA0","circuit breaker VL1250L very high breaking capacity Icu=100kA, 415V AC 3-pole, line protection trip unit ETU12, LIG 3 phases/3 lines In=1250A, rated current IR=500...1250A, overload protection, II=1.25 to 10xIN, short-circuit protection without auxiliary release ETU communication-capable without auxiliary/alarm switch",9500,"ST",1,"LP",1,"3VL77123ML360AA0"]
["3VL8716-2LB30-0AA0","circuit breaker VL1600H high breaking capacity Icu=70kA, 415V AC 3-pole, line protection trip unit ETU10, LI In=1600A, rated current IR=640...1600A, overload protection, II=1.25 to 9 xIN, short-circuit protection shipbuilding certificate for LRS, DNV and gL without auxiliary release without auxiliary/alarm switch",11098,"ST",1,"LP",1,"3VL87162LB300AA0"]
["3VL9100-4PA30","accessory for VL160X, plug-in base assembly kit rear connection, 3-pole",334,"ST",1,"LP",1,"3VL91004PA30"]
["3VL9200-4TB01","circuit br. VL std nut keeper D ACC cat. no. TNKD",13.299999999999999,"ST",1,"LP",1,"3VL92004TB01"]
["3VL9210-6LB30","ETU VL160 3-pole, line protection ETU10, LI IR=40...100A, overload protection, II=1.25 to 11xIN, short-circuit protection box terminal/screw terminal connections in scope of supply of sw. unit shipbuilding certificate for LRS, DNV and gL",532,"ST",1,"LP",1,"3VL92106LB30"]
["3VL9300-3JM01","accessory for VL150XUL, VL250UL (CG frame FG frame) Max Flex operator, complete incl. op. mech., lever and Bowden cable (length=0.9m)",872,"ST",1,"LP",1,"3VL93003JM01"]
["3VL9300-4TA31","accessory for VL250UL, (FG frame) connection with screw terminal metric thread comprises 3 connections",37.4,"ST",1,"LP",1,"3VL93004TA31"]
["3VL9325-5GF40","accessory for VL250, RCD module (RCD) In=250A Ue=230...690V, 4-pole",2004,"ST",1,"LP",1,"3VL93255GF40"]
["3VL9325-6ML30","ETU VL250 3-pole, line protection ETU12, LIG 3 phases/3 lines IR=100...250A, overload protection, II=1.25 to 11xIN, short-circuit protection screw terminal connections in scope of delivery of switching unit",1740,"ST",1,"LP",1,"3VL93256ML30"]
["3VL9400-3JS11","Breaker VLVAR DEPTH 1 3R 12 J/L-FR 3/4P",386,"ST",1,"LP",1,"3VL94003JS11"]
["3VL9400-4WC31","accessory for VL400UL, (JG frame) withdr. vers., assembly kit front connection, 3-pole",1646,"ST",1,"LP",1,"3VL94004WC31"]
["3VL9431-6UJ40","ETU VL400, 4-pole, line protection LCD ETU40, LI/LS/LSI IR=126...315A, overload protection, ISD=1.5 to 10xIR, II=11 xIN short-circuit protection, N protected screw terminal connections in scope of delivery of switching unit",3048,"ST",1,"LP",1,"3VL94316UJ40"]
["3VL9531-7DK30","ETU VL630, 3-pole, starter combination II=2000...4000A, short-circuit protection screw terminal conn. in scope of delivery of switching unit",561,"ST",1,"LP",1,"3VL95317DK30"]
["3VL9600-3HP02","accessory for VL630, VL800, fixing bracket for shaft of door-coupling rot. op. mech.","on request",null,null,"LP",1,"3VL96003HP02"]
["3VL9600-4WC40","accessory for VL800, withdr. vers., assembly kit front connection, 4-pole",2596,"ST",1,"LP",1,"3VL96004WC40"]
["3VL9775-4TG21","Breaker VL2-LUG Kit CU-AL 2W 7 CAT number 2TA3NG750",1157,"ST",1,"LP",1,"3VL97754TG21"]
["3VL9800-3JF01","Breaker VLHDL 3R VAR DEPTH red M/P-FR",147,"ST",1,"LP",1,"3VL98003JF01"]
["3VL9816-6TB40","ETU VL1600, 4-pole, line protection ETU10, LI IR=640...1600A, overload protection, II=1.25 to 9 xIN, short-circuit protection, screw terminal connections in scope of delivery of switching unit",7045,"ST",1,"LP",1,"3VL98166TB40"]
["3VL9875-4TH01","accessory for VL1600UL, (PG frame) multiple feed-in terminal for Cu/Al for 4 conductors per terminal 600-750 KCMIL f. inst. w/ mounting base",444,"ST",1,"LP",1,"3VL98754TH01"]
["3VT9100-2AB20","accessory for VT160 auxiliary switch 1CO VT160 5-60V AC/DC",35.300000000000004,"ST",1,"LP",1,"3VT91002AB20"]
["3VT9116-5GY42","accessory for VT160 connection set, long 4-pole",131,"ST",1,"LP",1,"3VT91165GY42"]
["3VT9300-3HE20","accessory for VT250, VT630 handle with locking black",21.200000000000003,"ST",1,"LP",1,"3VT93003HE20"]
["3VT9512-6AC00","ETU VT1600 3-pole, line protection ETU DP, LI IR=500...1250A, overload protection IRM=1.5...18kA, short-circuit protection, screw terminal connections in scope of delivery of switching unit",2405,"ST",1,"LP",1,"3VT95126AC00"]
["3VW9011-0AH07","mechanical op. cycles counter MOC accessory for circuit breaker 3WL10 / 3VA27 (SE)",152,"ST",1,"LP",1,"3VW90110AH07"]
["3VW9011-0AP13","protective cover IP54 hood lock with standard key for installing in cabinet door accessory for circuit breaker 3WL10 / 3VA27",119,"ST",1,"LP",1,"3VW90110AP13"]
["3VW9727-0VL10","locking device, OFF pos. Ronis against unauthorized closing for MCCB w/ rotary op. mech. accessory for circuit breaker 3VA27 (handle)",112,"ST",1,"LP",1,"3VW97270VL10"]
["3WA9111-0AX11","Accessory Circuit breaker 3WA, Rear horizontal main- connection, top or bottom, frame size 1 - up to 1000 A for circuit breaker in withdrawable design, 1 piece",20.5,"ST",1,"LP",1,"3WA91110AX11"]
["3WA9111-0EC61","Accessory circuit breaker 3WA, DIN rail adapter for CubicleBUS modules",9.4,"ST",1,"LP",10,"3WA91110EC61"]
["3WA9111-0EX02","Accessory circuit breaker 3WA, Option Plug  LSIG GFx  250 A Basic protective function LT, ST, INST and GF, Rated current 250 A (Ground fault protection with extended setting range)",723,"ST",1,"LP",1,"3WA91110EX02"]
["3WL9111-0AE13-0AA0","accessories circuit breaker 3WL undervoltage release, w.delay AC 50/60Hz 208-240V/DC 220-250V",872.91,"ST",1,"LP",1,"3WL91110AE130AA0"]
["3WL9111-0AT26-0AA0","accessories circuit breaker 3WL digital output module with rot. coding switches, relay outputs can be connected to cubicle bus",443,"ST",1,"LP",1,"3WL91110AT260AA0"]
["3WL9111-0BC02-0AA0","ready-made cabling f. cubicle bus module 1 m long",15.9,"ST",1,"LP",1,"3WL91110BC020AA0"]
["3WL9111-2AA54-0AA0","accessories circuit breaker 3WL rated current ref. module 500A f. ETU25, 27, 45, 55, 75, 76 approved to UL 489",332,"ST",1,"LP",1,"3WL91112AA540AA0"]
["3ZS1322-6CE13-0YB5","SIRIUS SIMOCODE ES V15.1 Premium, Floating license for one user; Engineering software, without SW, without docu., license key download, Class A, 6 languages (de,en,it, fr,sp,cn) Combo license parallel use of SIMOCODE ES 2007 and V15 for SIMOCODE pro, Online functions via system interface and PROFIBUS / PROFINET, Int. graphic editor (CFC-based) Executable in: Win 7 SP1 / Win 10 - 64-bit (Prof./Ultimate/Enterprise) / Win Server 2012 R2 StdE / 2016 - 64-bit, E-mail address required",1670,"ST",1,"CP",1,"3ZS13226CE130YB5"]
["3ZS1633-2XX03-0YB0","PCS7 block library for 3RW44 Soft Starter V9.0+SP1 Runtime AS blocks for Integration of Soft Starters 3RW44 in the process control system PCS7 with APL for the PCS 7 version V9.0+SP1 Runtime software for execution of the AS block in an automation system (single license) License without software and documentation Content: Set (1xDVD + 1x USB)",306,"ST",1,"CP",1,"3ZS16332XX030YB0"]
["4AM2342-5AV00-0EB0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,025 /0; UPRI(V):400+/-5%; USEC(V):42; ISEC(A):0,6; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:MOUNTING RAILS; EN 61558-2-6 >UL/CSA-RECOGNIZED< >SAFETY ISOLATING TRANSFORMER<",199,"ST",1,"CP",1,"4AM23425AV000EB0"]
["4AM4042-6MT10-0FA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,25 /0,85; UPRI(V):690+/-10%; USEC(V):230; ISEC(A):1,09; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREWS/MOUNTING RAILS; EN 61558-2-1, -2-2, -2-4 >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",503,"ST",1,"CP",1,"4AM40426MT100FA0"]
["4AM4642-5FT10-0FA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,4 /1,44; UPRI(V):500+/-5%; USEC(V):230; ISEC(A):1,74; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",302,"ST",1,"CP",1,"4AM46425FT100FA0"]
["4AM5242-5FJ10-0FD0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,475 /2,34; UPRI(V):500+/-5%; USEC(V):110; ISEC(A):4,32; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP54; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",640,"ST",1,"CP",1,"4AM52425FJ100FD0"]
["4AM5542-4TT10-0FA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,8 /3,4; UPRI(V):230+/-5%; USEC(V):230; ISEC(A):3,48; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",481,"ST",1,"CP",1,"4AM55424TT100FA0"]
["4AM5742-8JD40-0FD0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,75 /5; UPRI(V):400-230+/-15; USEC(V):2X115; ISEC(A):2X3,26; F(HZ):50...60; VECTOR GR./SHIELD WNG.:III0 /0; TA/ISOKL:40 /B; IP54; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",1553,"ST",1,"CP",1,"4AM57428JD400FD0"]
["4AT3032-5AT10-0FD0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):3,15 /16; UPRI(V):400+/-5%; USEC(V):230; ISEC(A):13,7; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:55 /H; IP54; TYPE OF TERMINALS:SCREW CONNECTION; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",2215,"ST",1,"CP",1,"4AT30325AT100FD0"]
["4AT3932-8DD40-0FA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):10 /30; UPRI(V):550-525-500-480-460- 440-415-400-380-230-208; USEC(V):2X115; ISEC(A):43,5-87,0; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:55 /H; IP00; TYPE OF TERMINALS:SCREW CONNECTION; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",4196,"ST",1,"CP",1,"4AT39328DD400FA0"]
["4BU5232-2AA20-2YC3","TRANSFORMER; PHASES:3; PN(KVA):40,5; UPRI(V):400; USEC(V):400 (LASTSPANNUNG/LOAD VOLTAGES); ISEC(A):58,5; F(HZ):50...60; VECTOR GR./SHIELD WNG.:DYN11 /0; TA/ISOKL:40 /H; IP23; TYPE OF TERMINALS:SCREW CONNECTION; INSTALLATION:PLACE; VDE 0532",23584,"ST",1,"CP",1,"4BU52322AA202YC3"]
["4BU5832-2AA20-2YC3","TRANSFORMER; PHASES:3; PN(KVA):100,5; UPRI(V):400; USEC(V):400 (LASTSPANNUNG/LOAD VOLTAGES); ISEC(A):145,1; F(HZ):50...60; VECTOR GR./SHIELD WNG.:DYN11 /0; TA/ISOKL:40 /H; IP23; TYPE OF TERMINALS:FLAT-TYPE TERMINAL; INSTALLATION:PLACE; VDE0532",38995,"ST",1,"CP",1,"4BU58322AA202YC3"]
["4EU2722-1CA00-0AA0","COMMUTATING CHOKE FOR CONVERTER; PHASES:3; UN1(V):500; ITHMAX 1(A) / F1(HZ):180 /50; I LN (A):162; UK(%):4; LN(MH):0,156; TA/ISOKL:40 /H; IP00; TYPE OF TERMINALS:FLAT-TYPE TERMINAL; EN 61558-2-20 >UL/CSA-RECOGNIZED< >CHOKE<",5603,"ST",1,"CP",1,"4EU27221CA000AA0"]
["4EU3652-3UB00-0AA0","MAINS CHOKE F.FU; PHASES:3; UN1(V):480; ITHMAX 1(A) / F1(HZ):400 /60; I LN (A):360; UK(%):4; LN(MH):0,0704; TA/ISOKL:40 /H; IP00; TYPE OF TERMINALS:FLAT-TYPE TERMINAL; EN 61558-2-20 >UL/CSA-RECOGNIZED< >CHOKE<",12474,"ST",1,"CP",1,"4EU36523UB000AA0"]
["4RB2025-3CD50","Power capacitor PHICAP MKP 230 V 2.5 kVAr","On request","ST",1,"LP",8,"4RB20253CD50"]
["4RB2167-3EA50","Power capacitor PHICAP MKP 400 V 16.7 kVAr","On request","ST",1,"LP",8,"4RB21673EA50"]
["4RB3100-3FC50","Power capacitor MKV MKV 525 V 10.0 kVAr",1318.37,"ST",1,"LP",2,"4RB31003FC50"]
["4RB5050-3GK50","Power capacitor PHASECAP MKK 690 V 5.0 kVAr","On request","ST",1,"LP",8,"4RB50503GK50"]
["4RF1704-3NB04","7% choked control unit in sheet-steel cabinet IP20 Basic unit with controller 40kVAr 400V 50Hz Number of stages 4x 10 kVAr Control series 1111 Other rated voltages on request",22182.799999999999,"ST",1,"LP",1,"4RF17043NB04"]
["4RF5610-3GA42-2","5.67% choked capacitor module for cabinet width 800 mm for cabinet depth 600 mm with MKK capacitors Control line connector with fuse Switch disconnector fronts. Busbar 30x 10 mm 100kVAr 400V 50Hz can be switched as 1x 100 kVAr Other rated voltages on request",16153.38,"ST",1,"LP",1,"4RF56103GA422"]
["4RF6740-2AE40-2","7% choked fixed compensation for three-phase current connection in sheet-steel enclosure Degree of protection IP20 with discharge unit 40kVAr 400V 50Hz Other rated voltages on request",8279.19,"ST",1,"LP",1,"4RF67402AE402"]
["4RY5805-6GA47","Unchoked capacitor module for cabinet width 800 mm for cabinet depth 400 mm with MKK capacitors with discharge unit with fuse Switch disconnector fronts. Busbar 30x 10 mm 50kVAr 690V 50Hz Can be switched as 1x 50 kVAr",6479.37,"ST",1,"LP",1,"4RY58056GA47"]
["5SD7448-1","Plug-in part type 1 L-N Requirement class B, UC 350V 1-pole for combi-arrester 5SD744",214,"ST",1,"LP",1,"5SD74481"]
["5SE2350","NEOZED fuse-link, D02, 50 A, gG, Un AC: 400 V, Un DC: 250 V, with silver-coated contact-caps",0.92,"ST",1,"LP",10,"5SE2350"]
["5SH327","DIAZED screw adapter insert DIII 32A",1.28,"ST",1,"LP",25,"5SH327"]
["5SJ4132-7HG40","Miniature circuit breaker 240 V 14kA, 1-pole, C, 32 A, D=70 mm according to UL 489, equal polarity",167,"ST",1,"LP",1,"5SJ41327HG40"]
["5SJ4210-8HG42","Circuit breaker 10kA, 2-pole, D, 10 A according to UL 489-480Y/277V",522,"ST",1,"LP",1,"5SJ42108HG42"]
["5SJ4308-8HG41","Miniature circuit breaker 240 V 4 kA, 3-pole, D, 8A, D=70 mm according to UL 489",922,"ST",1,"LP",1,"5SJ43088HG41"]
["5SL3008-7KL","CIRCUIT BREAKER 230V 4.5KA, 1+N-POLE/1MW, N LEFT C8","Please order 5SL6008-7KL","ST",1,"LP",1,"5SL30087KL"]
["5SL3525-6","Miniature circuit breaker 230 V 4.5 kA, 1+N-pole, B, 25A","Please order 5SL6525-6","ST",1,"LP",1,"5SL35256"]
["5SL4150-8","Miniature circuit breaker 230/400 V 10kA, 1-pole, D, 50 A",18.3,"ST",1,"LP",1,"5SL41508"]
["5SL4316-8","Miniature circuit breaker 400 V 10kA, 3-pole, D, 16A",46.300000000000004,"ST",1,"LP",1,"5SL43168"]
["5SL4608-8","Miniature circuit breaker 400 V 10kA, 3+N-pole, D, 8A",70.099999999999994,"ST",1,"LP",1,"5SL46088"]
["5SL6101-7","Miniature circuit breaker 230/400 V 6kA, 1-pole, C, 1 A",4.96,"ST",1,"LP",1,"5SL61017"]
["5SL6225-7","Miniature circuit breaker 400 V 6kA, 2-pole, C, 25A",12.7,"ST",1,"LP",1,"5SL62257"]
["5SM2345-6KK01","RC unit for 5SY, 4-pole, type A, short-time delayed, In: 63 A, 30 mA, Un AC: 400 V",321,"ST",1,"LP",1,"5SM23456KK01"]
["5SM3318-6KK","Residual current operated circuit breaker, 2-pole, type A, In: 100 A, 30 mA, Un AC: 230 V",444,"ST",1,"LP",1,"5SM33186KK"]
["5SP3250-3","Main miniature circuit breaker (SHU), 2-pole, E 50, 400V",505,"ST",1,"LP",1,"5SP32503"]
["5ST1315","busbar adapter for Main miniature circuit breaker (SHU), for 40 mm clearance with infeed terminals",82.13000000000001,"ST",1,"LP",1,"5ST1315"]
["5ST3612","Pin busbar, 10 mm2 connection: 5x (2-phase+AUX/FS) touch-safe",4.5,"ST",1,"LP",10,"5ST3612"]
["5ST3704","Pin busbar touch-safe, 16 mm2 2-phase, 214 mm long can be cut, with end caps",9.75,"ST",1,"LP",1,"5ST3704"]
["5ST3741","Pin busbar touch-safe, 10 mm2 3-phase+AUX, 214 mm long can be cut, with end caps",9.32,"ST",1,"LP",1,"5ST3741"]
["5SU1324-7KX10","RCBO, Icn: 10 kA, 2P, type A, 30 mA, C-Char, In: 10 A, Un AC: 110 V",226,"ST",1,"LP",1,"5SU13247KX10"]
["5SU1354-0KK06","RCBO, 10 kA, 1P+N, Type AC, 30 mA, B char., In: 6 A, Un AC: 230 V",437,"ST",1,"LP",1,"5SU13540KK06"]
["5SU1354-6GV16","RCBO, Icn: 10 kA, 1P+N, type A, 30 mA, B char., In: 16 A, Un AC: 230 V, bulk packaging",182,"ST",1,"LP",36,"5SU13546GV16"]
["5SU1654-0KK16","RCBO, 10 kA, 1P+N, Type AC, 300 mA, B char., In: 16 A, Un AC: 230 V",431,"ST",1,"LP",1,"5SU16540KK16"]
["5SU9354-8KK10","RCBO, 10 kA, 1P+N, type A, 30 mA, D char., In: 10 A, Un AC: 230 V",280,"ST",1,"LP",1,"5SU93548KK10"]
["5SU9356-7KP20","RCBO, 6 kA, 1P+N, type A, 30 mA, C-Char, In: 20 A, Un AC: 230 V, pigtail 300 mm",111,"ST",1,"LP",1,"5SU93567KP20"]
["5SV1616-6KK13","RCBO compact 1P+N 6 kA type A 300 mA B13",174,"ST",1,"LP",1,"5SV16166KK13"]
["5SV3614-8KL","Residual current operated circuit breaker, 2-pole, type A, selective, In: 40 A, 300 mA, Un AC: 230 V, N left",156,"ST",1,"LP",1,"5SV36148KL"]
["5SV4111-0KL","Residual current operated circuit breaker, 2-pole, Type AC, In: 16 A, 10 mA, Un AC: 230 V, N left",66.5,"ST",1,"LP",1,"5SV41110KL"]
["5SV4446-0LA","Residual current operated circuit breaker, 4-pole, Type AC, In: 63 A, 100 mA, Un AC: 400 V, with thermal overload protection",175,"ST",1,"LP",1,"5SV44460LA"]
["5SV6016-7KK06","AFDD-MCB-Combination 230V, 6kA, 1+N, C, 6A Compact (1MW)",225,"ST",1,"LP",1,"5SV60167KK06"]
["5SY4101-5","Miniature circuit breaker 230/400 V 10kA, 1-pole, A, 1 A, D=70 mm",34.800000000000004,"ST",1,"LP",1,"5SY41015"]
["5SY4132-7KK11","Miniature circuit breaker 230/400 V 10kA, 1-pole, C, 32A for railway applications",241.60999999999999,"ST",1,"LP",1,"5SY41327KK11"]
["5SY4245-7","Miniature circuit breaker 400 V 10kA, 2-pole, C, 45 A, D=70 mm",35.9,"ST",1,"LP",1,"5SY42457"]
["5SY4263-8","Miniature circuit breaker 400 V 10kA, 2-pole, D, 63 A, D=70 mm",173,"ST",1,"LP",1,"5SY42638"]
["5SY4410-6KK11","Miniature circuit breaker 400 V 10kA, 4-pole, B, 10 A for railway applications",841.41,"ST",1,"LP",1,"5SY44106KK11"]
["5SY4514-7","Miniature circuit breaker 230 V 10kA, 1+N-pole, C, 0.3A, D=70 mm",20.400000000000002,"ST",1,"LP",1,"5SY45147"]
["5SY4615-7","Miniature circuit breaker 400 V 10kA, 3+N-pole, C, 1.6 A, D=70 mm",51.300000000000004,"ST",1,"LP",1,"5SY46157"]
["5SY5263-6","Circuit breaker Universal current 440 V DC 400 V AC 10kA, 2-pole, B, 63A",174,"ST",1,"LP",1,"5SY52636"]
["5SY6010-7KL","Miniature circuit breaker 230 V 6kA, 1+N-pole/1 MW, N left C 10 A",26.1,"ST",1,"LP",1,"5SY60107KL"]
["5SY6406-7","Miniature circuit breaker 400 V 6kA, 4-pole, C, 6 A, D=70 mm",61.2,"ST",1,"LP",1,"5SY64067"]
["5SY7214-7","Miniature circuit breaker 400 V 15kA, 2-pole, C, 0.3A, D=70 mm",44.4,"ST",1,"LP",1,"5SY72147"]
["5SY7406-6","Miniature circuit breaker 400 V 15kA, 4-pole, B, 6 A, D=70 mm",89.199999999999989,"ST",1,"LP",1,"5SY74066"]
["5SY7625-7","Miniature circuit breaker 400 V 15kA, 3+N-pole, C, 25A, D=70 mm",66.5,"ST",1,"LP",1,"5SY76257"]
["5SY8102-8","Circuit breaker 230/400 V D=70 mm 25 kA according to EN 60947-2, 1P, D2",39.1,"ST",1,"LP",1,"5SY81028"]
["5SY8505-8","Miniature circuit breaker 230 V D=70 mm 25 kA according to EN 60947-2, 1P+N, D0.5",74.5,"ST",1,"LP",1,"5SY85058"]
["5SY8663-7","Miniature circuit breaker 400 V D=70 mm 25 kA according to EN 60947-2, 3P+N, C63",182,"ST",1,"LP",1,"5SY86637"]
["5TA5502-0MB","MEGA HotelCard switch 1, 2-way 1 microswitch Complete unit with Cover plate Misty bronze","On request","ST",1,"LP",1,"5TA55020MB"]
["5TD2120","DELTA pushbutton device insert, UP 1 NO, 10A 250V",9.7100000000000009,"ST",1,"LP",1,"5TD2120"]
["5TE4804","button, 1 NO+1 NO 20 A, 2 keys green blue Lamps 24 V",26.5,"ST",1,"LP",1,"5TE4804"]
["5TE5820","Indicator light 1 lamp 230 V red Lamp cannot be replaced",4.7699999999999996,"ST",1,"LP",1,"5TE5820"]
["5TG1125-3","DELTA miro aluminum Frame 5-fold Authentic material aluminum oxide yellow Dimensions 347x 90 mm",265,"ST",1,"LP",1,"5TG11253"]
["5TG1912","DELTA profil, titanium white Module rack, double incl. intermediate frame Screw mounting",9.34,"ST",1,"LP",1,"5TG1912"]
["5TG2552-8","DELTA line, carbon metallic frame 2-fold, 151x 80 mm vertical, with Labeling field",22.200000000000003,"ST",1,"LP",1,"5TG25528"]
["5TG2901","DELTA line/Style Surface-mounting enclosure, 1 x titanium white",15.4,"ST",1,"LP",1,"5TG2901"]
["5TG5530-0MA","IRIS Rocker switch Alaska aluminum",10.1,"ST",1,"LP",1,"5TG55300MA"]
["5TG5533-5MA","IRIS Cover plate 40 mm for loudspeaker socket and presence detector Alaska aluminum",12.1,"ST",1,"LP",1,"5TG55335MA"]
["5TG5535-5MA","IRIS Cover plate for TAE connection socket and loudspeaker connection socket Mercury aluminum",17.600000000000001,"ST",1,"LP",1,"5TG55355MA"]
["5TG5542-0MG","MEGA Cover plate for Pushbutton 2-fold, switch for shutter with symbols Up, Down malt gold","On request","ST",1,"LP",1,"5TG55420MG"]
["5TG6220-1","DELTA i-system piano black Rocker switch with window for device inserts Universal switch, button, etc. 55x 55 mm",20.400000000000002,"ST",1,"LP",1,"5TG62201"]
["5TG6251","DELTA i-system aluminum-metallic Rocker switch with window, with label for emergency switch for heating 55x 55 mm",8.6,"ST",1,"LP",1,"5TG6251"]
["5TG8058-3","LED lamp Green 230 V",4.0999999999999996,"ST",1,"LP",5,"5TG80583"]
["5TL1291-0","off switch 100A 2-pole",24.400000000000002,"ST",1,"LP",1,"5TL12910"]
["5TT4456-0","Remote control switch Contact for 32 A Voltage 230 V AC 2 NO 2 NC",52.800000000000004,"ST",1,"LP",1,"5TT44560"]
["5TT5042-0","INSTA contactor with 2 NO contacts and 2 NC Contact for 230 V AC, 400V 40A Control 230 V AC 220 V DC",93.6,"ST",1,"LP",1,"5TT50420"]
["5UB1367","DELTA style, titanium white Socket outlet 10/16A 250 V with grounding pin with increased touch protection 2-pole according to CEE7 cover plate 68 x 68 mm",20.200000000000003,"ST",1,"LP",1,"5UB1367"]
["5UB1905","DELTA i-system electrical white SCHUKO socket outlet 10/16 A 250 V With screwless Connection terminals with spring flap 55x 55 mm and increased touch protection",20.5,"ST",1,"LP",1,"5UB1905"]
["5UH1055","DELTA profil, silver Cover plate 65x 65 mm with bezel black for SCHUKO socket outlet",13.4,"ST",1,"LP",1,"5UH1055"]
["7KM5412-6BA00-1EA2","SENTRON, meas. device & power quality recorder, 7KM PAC5200, LCD, L-L: 690 V, L-N: 400 V, 10 A, 3-phase, Modbus TCP, apparent/active/reactive energy / cos phi, harmonics: 2.-40., THD, class 0.5 acc. to IEC61557-12 or cl. 0.5S acc. to IEC62053-22, wide-range pwr sup. unit AC/DC, screw terminals",3610,"ST",1,"LP",1,"7KM54126BA001EA2"]
["7PV1508-1AW30","Timing relay, electronic Multifunction 1 change-over contact, 7 functions 7 time ranges 0.05 s ... 100 h 12-240 V AC/DC with LED, Screw terminal",63.800000000000004,"ST",1,"CP",1,"7PV15081AW30"]
["8GB2052-1","SIMBOX Universal WP N/PE terminal strip 2x3x 25 mm2+2x10x 10 mm2",17.200000000000003,"ST",1,"LP",1,"8GB20521"]
["8GF9683","Stab Universal Terminal strip vertical (Mounting on mounting rail)",19.600000000000001,"ST",1,"LP",1,"8GF9683"]
["8GK1052-5KK41","ALPHA 160, wall-mounted cabinet, Surface mounting, with distribution board panel, IP44, Protection class 2, H: 1100 mm, W: 1050 mm, T: 140 mm, RAL 9016",1358,"ST",1,"LP",1,"8GK10525KK41"]
["8GK1302-8KK42","ALPHA 630, Floor-mounted cabinet, Flat Pack, IP43, Protection class 1, H: 1900 mm, W: 1050 mm, T: 210 mm, RAL 7035",1295,"ST",1,"LP",1,"8GK13028KK42"]
["8GK1423-8KK25","ALPHA 1250, Floor-mounted cabinet, with open side wall, IP55, Protection class 1, H: 1950 mm, W: 550 mm, T: 400 mm, RAL 7035","On request","ST",1,"LP",1,"8GK14238KK25"]
["8GK2300-6KL23","ALPHA 630 UNIVERSAL, Floor-mounted cabinet, Flat Pack, IP43, Protection class 1, H: 1800 mm, W: 600 mm, T: 250 mm, RAL 7035, without door",477,"ST",1,"LP",1,"8GK23006KL23"]
["8GK4402-4KK22","ALPHA 400/630 DIN, Assembly kit Modular terminal blocks with terminal strip Section cover closed vertical, H=600 W=500",224,"ST",1,"LP",1,"8GK44024KK22"]
["8GK4710-3KK10","ALPHA 400/630 assembly kit 3VT 2 3VT2 molded case circuit breaker up to 250 A, Fixed mounting on support plate H=450/W=250",161,"ST",1,"LP",1,"8GK47103KK10"]
["8GK4853-8KK02","ALPHA 630/1600 DIN longitudinal stays 2 units longitudinal stays, H=1800 mm for depth 250/320 mm",102,"SZ",1,"LP",1,"8GK48538KK02"]
["8GK6714-6KK23","ALPHA 630 Universal, Circuit breaker kit 1x 3VL630 3+4-pole H=600 mm W=600 mm, horizontal Installation",186,"ST",1,"LP",1,"8GK67146KK23"]
["8GK6750-6KK13","ALPHA 630 Universal Circuit breaker kit 1x 3VT2 3+4-pole H=600 mm W=250 mm for cable compartment",177,"ST",1,"LP",1,"8GK67506KK13"]
["8GK9507-8KK20","ALPHA 630 Universal, Door IP55, Transparent (Giugiaro design), RAL 7035, H=1600, W=600",488,"ST",1,"LP",1,"8GK95078KK20"]
["8GK9511-8KK32","ALPHA, door half, on the right, IP31, H: 1250 mm, W: 275 mm, RAL 9016, type of protection 1 and 2",127,"ST",1,"LP",1,"8GK95118KK32"]
["8GK9607-5KK10","ALPHA 630 Universal, Section cover without cutouts H=800 mm W=300 mm",68.599999999999994,"ST",1,"LP",1,"8GK96075KK10"]
["8GK9901-0KA12","ALPHA, Base, H: 100 mm, W: 300 mm, T: 210 mm, RAL 7035",149,"ST",1,"LP",1,"8GK99010KA12"]
["8GK9910-0KK80","ALPHA 400/630 wiring clip on standard mounting rail Minimum order quantity 200 units",1.68,"ST",1,"LP",200,"8GK99100KK80"]
["8GS4016-1","ALPHA-ZS, Quick assembly kit for telecommunications, H=900, W=250 with perforated sheet and insert nut","On request","ST",1,"LP",1,"8GS40161"]
["8JH4104","Terminal 1-pole, for bar 12x 5 Conductor connection 1x 16-35 mm2","On request","ST",1,"LP",10,"8JH4104"]
["8MF1000-2UW62-1B","SIVACON, side panel / rear panel, Closed, EMC, IP40, H: 2000 mm, W: 1000 mm, RAL 7035",1168,"ST",1,"LP",1,"8MF10002UW621B"]
["8MF1005-2VH","SIVACON, roof trough, IPX1, W: 1000 mm, D: 500 mm, RAL 7035",230,"ST",1,"LP",1,"8MF10052VH"]
["8MF1020-2AA02-0","SIVACON, mounting plate, Quick assembly with screws, H: 1000 mm, W: 1200 mm, zinc-plated",252,"ST",1,"LP",1,"8MF10202AA020"]
["8MF1040-2AF20","SIVACON, compartment bottom, T: 1000 mm, W: 400 mm, zinc-plated",268,"ST",1,"LP",1,"8MF10402AF20"]
["8MF1045-2UB22-0","SIVACON, base, IP30, T: 500 mm, W: 400 mm, zinc-plated",61.6,"ST",1,"LP",1,"8MF10452UB220"]
["8MF1060-2UT15-3BA2","SIVACON, door, left, with cutout for filter fan, with ventilation openings H: 2000 mm, W: 600 mm, RAL 7035, Protection class 1",678,"ST",1,"LP",1,"8MF10602UT153BA2"]
["8MF1060-2UT25-0CA1","SIVACON, door half, left, EMC, IP40, H: 2000 mm, W: 600 mm, RAL 7035, Protection class 1",1188,"ST",1,"LP",1,"8MF10602UT250CA1"]
["8MF1080-2UT15-3BA2","SIVACON, door, left, with cutout for filter fan, with ventilation openings H: 2000 mm, W: 800 mm, RAL 7035, Protection class 1",722,"ST",1,"LP",1,"8MF10802UT153BA2"]
["8MF1086-2UB52-0","SIVACON, base, with cutouts for flanges, IPXX, T: 600 mm, W: 800 mm, zinc-plated",106,"ST",1,"LP",1,"8MF10862UB520"]
["8MF1090-2HC13-0","SIVACON, mounting rail, serrated, L: 900 mm, zinc-plated",43.4,"ST",1,"LP",1,"8MF10902HC130"]
["8MF1111-0AA00-0AB5","SIVACON 2000mm x 600mm x 500mm",2920,"ST",1,"LP",1,"8MF11110AA000AB5"]
["8MF1111-0AA00-0AL5","SIVACON 2000mm x 600mm x 500mm",1058,"ST",1,"LP",1,"8MF11110AA000AL5"]
["8MF1111-0AA00-0AR6","SIVACON 2000mm x 800mm x 800mm",4920,"ST",1,"LP",1,"8MF11110AA000AR6"]
["8MF1111-0AA00-0BP4","SIVACON 2000mm x 800mm x 400mm",3520,"ST",1,"LP",1,"8MF11110AA000BP4"]
["8MF1111-0AA00-0CA8","SIVACON 2000mm x 600mm x 800mm",3660,"ST",1,"LP",1,"8MF11110AA000CA8"]
["8MF1111-0AA00-0CE3","SIVACON 2000mm x 800mm x 600mm",5680,"ST",1,"LP",1,"8MF11110AA000CE3"]
["8MF1111-0AA00-0CS0","SIVACON 2200mm x 900mm x 600mm",2320,"ST",1,"LP",1,"8MF11110AA000CS0"]
["8MF1111-0AA00-0DQ0","SIVACON 2000mm x 800mm x 600mm",3520,"ST",1,"LP",1,"8MF11110AA000DQ0"]
["8MF1111-0AA00-0EA0","SIVACON 2000mm x 600mm x 500mm",2980,"ST",1,"LP",1,"8MF11110AA000EA0"]
["8MF1111-0AA00-0EG7","SIVACON 1800mm x 1200mm x 400mm",4060,"ST",1,"LP",1,"8MF11110AA000EG7"]
["8MF1111-0AA00-0ES5","SIVACON 1800mm x 600mm x 400mm",3540,"ST",1,"LP",1,"8MF11110AA000ES5"]
["8MF1111-0AA00-0FL0","SIVACON 2000mm x 1200mm x 600mm",5880,"ST",1,"LP",1,"8MF11110AA000FL0"]
["8MF1111-0AA00-0FQ7","SIVACON 1800mm x 600mm x 600mm",3520,"ST",1,"LP",1,"8MF11110AA000FQ7"]
["8MF1111-0AA00-0GE1","SIVACON 2200mm x 1000mm x 800mm",3720,"ST",1,"LP",1,"8MF11110AA000GE1"]
["8MF1228-3BR5","SIVACON, Control panel Empty enclosure, without side panels, according to IEC 62208, IP55, H: 2200 mm, W: 1200 mm, T: 800 mm",4020,"ST",1,"LP",1,"8MF12283BR5"]
["8MF1250-2HL6","SIVACON, cable channel, L: 2000 mm, H: 50 mm, W: 50 mm",77,"ST",1,"LP",1,"8MF12502HL6"]
["8MF1260-2UT25-0BA2","SIVACON, door half, left, IP55, H: 2200 mm, W: 600 mm, RAL 7035, Protection class 1",530,"ST",1,"LP",1,"8MF12602UT250BA2"]
["8MF1280-2UT14-0CA1","SIVACON, door, right, EMC, IP40, H: 2200 mm, W: 800 mm, RAL 7035, Protection class 1",1398,"ST",1,"LP",1,"8MF12802UT140CA1"]
["8MF1360-2HH","SIVACON, cable propping bar, H: 30 mm, W: 600 mm, zinc-plated",26,"ST",1,"LP",1,"8MF13602HH"]
["8MF1800-3BR4","SIVACON, Control panel Empty enclosure, without side panels, according to IEC 62208, IP40, H: 1800 mm, W: 1000 mm, T: 1000 mm",3420,"ST",1,"LP",1,"8MF18003BR4"]
["8MF1824-3BS4","SIVACON, Control panel Empty enclosure, according to IEC 62208, IP40, H: 1800 mm, W: 1200 mm, T: 400 mm",3780,"ST",1,"LP",1,"8MF18243BS4"]
["8MF1860-2UT15-1BA2","SIVACON, door, left, ventilated, IP20, H: 1800 mm, W: 600 mm, RAL 7035, Protection class 1",660,"ST",1,"LP",1,"8MF18602UT151BA2"]
["8MF1866-3BR5","SIVACON, Control panel Empty enclosure, without side panels, according to IEC 62208, IP55, H: 1800 mm, W: 600 mm, T: 600 mm",2500,"ST",1,"LP",1,"8MF18663BR5"]
["8MF1890-2UT25-0BA2","SIVACON, door half, left, IP55, H: 1800 mm, W: 900 mm, RAL 7035, Protection class 1",596,"ST",1,"LP",1,"8MF18902UT250BA2"]
["8MF2096-4EN","SICUBE 8MF 2000 EMC cabinet, welding version NI HxWxD=2000x 900x 600 mm for stand-alone installation with side panels, IP40","On request","ST",1,"LP",1,"8MF20964EN"]
["8MF2286-3RB","standard cabinet 8MF2 HxWxD=2200x 800x 600 Installation: Side-by-side ventilated, mounted, welded IP30","On request","ST",1,"LP",1,"8MF22863RB"]
["8MF2804-5R","standard cabinet 8MF2 HxWxD=1800x 1000x 400 Installation: Side-by-side non-ventilated, assembled, welded IP54,","On request","ST",1,"LP",1,"8MF28045R"]
["8MF2894-4EN","SICUBE 8MF 2000 EMC cabinet, welding version NI HxWxD=1800x 900x 400 mm for stand-alone installation with side panels, IP40","On request","ST",1,"LP",1,"8MF28944EN"]
["8MF3066-8","compartment door instead of a standard door HxW=2000x 800","On request","ST",1,"LP",1,"8MF30668"]
["8MF3401","SIVACON, roof, with ventilation openings IP20, W: 600 mm, D: 600 mm, RAL 7032","On request","ST",1,"LP",1,"8MF3401"]
["8MF3498","SIVACON, roof, with cable gland, IP40, W: 1200 mm, D: 800 mm, RAL 7032","On request","ST",1,"LP",1,"8MF3498"]
["8MF4051","Transport rollers H=85 mm for 8MF cabinet accessories","On request","ST",1,"LP",1,"8MF4051"]
["8MF4270","Trim strip with Siemens logo petrol and drilled hole for lamp","On request","ST",1,"LP",1,"8MF4270"]
["8MF4801","standard compartment bottom mounted stationary HxD=600x 600","On request","ST",1,"LP",1,"8MF4801"]
["8MF4881","19-inch swing frame 6 HU","On request","ST",1,"LP",1,"8MF4881"]
["8MF5868-4E","Standard cabinet 8MF5 HxWxD=1800x 600x 800 Installation: single non-ventilated, not mounted, screwed IP40","On request","ST",1,"LP",1,"8MF58684E"]
["8MF6088-4ES","EMC cabinet IP40 HxWxD=2000x 800x 800","On request","ST",1,"LP",1,"8MF60884ES"]
["8MF6284-4ES","EMC cabinet IP40 HxWxD=2200x 800x 400","On request","ST",1,"LP",1,"8MF62844ES"]
["8MF6896-5E","Standard cabinet 8MF6 HxWxD=1800x 900x 600 Installation: single non-ventilated, assembled, welded IP54,","On request","ST",1,"LP",1,"8MF68965E"]
["8MR2170-1AF","Electronic hygrostat EFR012 230 V AC, 40-90 %RF","On request","ST",1,"LP",1,"8MR21701AF"]
["8MR6323-5DL42","Roof fan, Extract: W: 345 mm, H: 265 mm, RAL 7035, IP54, Airflow: 690 m3/h, Ue AC: 230 V","On request","ST",1,"LP",1,"8MR63235DL42"]
["8MR6500-5GV67","Outlet filter, Extract: W: 191 mm, H: 191 mm, RAL 7035, IP55","On request","ST",1,"LP",1,"8MR65005GV67"]
["8PQ1204-4BA08","SIKUS 1600, modular distribution board, IP55, H: 2000 mm, W: 400 mm, D: 400 mm",1061.9100000000001,"ST",1,"LP",1,"8PQ12044BA08"]
["8PQ2015-6BA10","SIVACON S4, mod door, IP40, H: 150mm, W: 600mm",115,"ST",1,"LP",1,"8PQ20156BA10"]
["8PQ2020-8BA23","SIVACON S4 mod door 3VA20(100A) 3VA21 (160A) 3VA22 (250A) fixed-mounted, plug-in tech. H: 200 mm W: 800 mm",190,"ST",1,"LP",1,"8PQ20208BA23"]
["8PQ2040-6BA06","SIVACON S4 cover 3VL5 up to 630A 3-pole fixed-mounted plug-in socket H:400mm W: 600mm",146,"ST",1,"LP",1,"8PQ20406BA06"]
["8PQ2050-8BA12","SIVACON S4 cover 3VA12 (250A), 3-pole, fixed-mounted, H: 500mm W: 800mm",180,"ST",1,"LP",1,"8PQ20508BA12"]
["8PQ2060-0BA06","SIVACON S4, mod door, IP40, H: 625 mm, W: 850 mm",312,"ST",1,"LP",1,"8PQ20600BA06"]
["8PQ2080-0BA07","SIVACON S4 inner door strut for H: 800mm",35.9,"ST",1,"LP",1,"8PQ20800BA07"]
["8PQ2197-8BA11","SIVACON S4 frame paneling IP30 W: 800mm",257,"ST",1,"LP",1,"8PQ21978BA11"]
["8PQ2304-4BA15","SIVACON S4 top plate MBB: rear IPX1 W: 400mm D: 400mm",106,"ST",1,"LP",1,"8PQ23044BA15"]
["8PQ2420-0BA01","SIVACON S4 rear wall, IP40, W: 350mm",177,"ST",1,"LP",1,"8PQ24200BA01"]
["8PQ3000-0BA82","SIVACON S4 plug-in strip H: 1600mm",105,"ST",1,"LP",1,"8PQ30000BA82"]
["8PQ3000-3BA43","SIVACON S4 MBB separation bottom with cable entry, W: 800mm D: 800mm",214,"ST",1,"LP",1,"8PQ30003BA43"]
["8PQ4000-2BA22","SIVACON S4 N/PE connection cable compartment",57.4,"ST",1,"LP",1,"8PQ40002BA22"]
["8PQ5000-2BA30","SIVACON S4 separation lateral, 100 - 250A, H: 200mm",45.4,"ST",1,"LP",1,"8PQ50002BA30"]
["8PQ5000-4BA73","SIVACON S4 basic module separation, rear H:=150mm W:=600mm",38.200000000000003,"ST",1,"LP",1,"8PQ50004BA73"]
["8PQ5000-5BA53","SIVACON S4 separation rear 1 x ACB MBB: single W: 600mm D: 1000mm",305,"ST",1,"LP",1,"8PQ50005BA53"]
["8PQ6000-3BA12","SIVACON S4 mounting panel 3VL7-8 1250A 1600A 3-pole 4-pole fixed-mounted H:700mm W: 600mm",215,"ST",1,"LP",1,"8PQ60003BA12"]
["8PQ6000-5BA72","SIVACON S4 cable connection 3NP1143 (NH1 up to 250A)",165,"ST",1,"LP",1,"8PQ60005BA72"]
["8PQ6000-8BA47","SIVACON S4 mounting panel 3VA10 (100A), 3-pole, fixed-mounted, plug-in socket,H:350mm W:800mm",146,"ST",1,"LP",1,"8PQ60008BA47"]
["8PQ9100-1AA40","partition","On request","ST",1,"LP",10,"8PQ91001AA40"]
["8PQ9100-8AA03","end mask w04","On request","ST",1,"LP",20,"8PQ91008AA03"]
["8PQ9103-3AA58","beam","On request","ST",1,"LP",10,"8PQ91033AA58"]
["8PQ9105-1AA51","partition","On request","ST",1,"LP",1,"8PQ91051AA51"]
["8PQ9105-8AA75","partition","On request","ST",1,"LP",1,"8PQ91058AA75"]
["8PQ9106-1AA30","reinforcement","On request","ST",1,"LP",100,"8PQ91061AA30"]
["8PQ9107-2AA38","base plate 10x04","On request","ST",1,"LP",1,"8PQ91072AA38"]
["8PQ9107-4AA04","cover for main busbar rear","On request","ST",1,"LP",1,"8PQ91074AA04"]
["8PQ9107-8AA24","compartment door plate w04 h0775","On request","ST",1,"LP",1,"8PQ91078AA24"]
["8PQ9108-0AA48","partition","On request","ST",1,"LP",1,"8PQ91080AA48"]
["8PQ9110-4AA04","supporting bracket w12","On request","ST",1,"LP",1,"8PQ91104AA04"]
["8PQ9110-6AA57","Terminal block HC-KA-D-40-BU-TWIN-2.5-8-S-R","On request","ST",1,"LP",10,"8PQ91106AA57"]
["8PQ9112-8AA70","partition w400","On request","ST",1,"LP",1,"8PQ91128AA70"]
["8PQ9113-3AA42","mounting plate h1000 w1000","On request","ST",1,"LP",1,"8PQ91133AA42"]
["8PQ9114-6AA17","base plate","On request","ST",1,"LP",1,"8PQ91146AA17"]
["8PQ9115-0AA22","partition","On request","ST",1,"LP",1,"8PQ91150AA22"]
["8PQ9117-1AA56","partition","On request","ST",1,"LP",1,"8PQ91171AA56"]
["8PQ9121-1AA11","plate","On request","ST",1,"LP",1,"8PQ91211AA11"]
["8PQ9122-8AA00","bracket 2 left","On request","ST",1,"LP",1,"8PQ91228AA00"]
["8PQ9123-8AA04","barrier d08 without lug MBB 4x30x10","On request","ST",1,"LP",10,"8PQ91238AA04"]
["8PQ9126-0AA63","Label","On request","ST",1,"LP",20,"8PQ91260AA63"]
["8PQ9127-4AA45","holder","On request","ST",1,"LP",1,"8PQ91274AA45"]
["8PQ9128-8AA32","bracket  DIN holder configuration","On request","ST",1,"LP",1,"8PQ91288AA32"]
["8PQ9131-8AA76","compartment door w06 h07","On request","ST",1,"LP",1,"8PQ91318AA76"]
["8PQ9133-6AA42","field door plate w08 h2175","On request","ST",1,"LP",1,"8PQ91336AA42"]
["8PQ9135-8AA71","cover","On request","ST",1,"LP",1,"8PQ91358AA71"]
["8PQ9136-8AA82","compartment door plate w08 h0775","On request","ST",1,"LP",1,"8PQ91368AA82"]
["8PQ9142-5AA55","cover d06 2x30","On request","ST",1,"LP",1,"8PQ91425AA55"]
["8PQ9143-5AA25","partition","On request","ST",1,"LP",1,"8PQ91435AA25"]
["8PQ9143-7AA18","partition w08","On request","ST",1,"LP",1,"8PQ91437AA18"]
["8PQ9146-7AA08","top plate duct LI w06 d06","On request","ST",1,"LP",1,"8PQ91467AA08"]
["8PQ9148-5AA60","Bracket for latch height 143","On request","ST",1,"LP",1,"8PQ91485AA60"]
["8PQ9150-4AA63","cover","On request","ST",1,"LP",1,"8PQ91504AA63"]
["8PQ9151-0AA25","device holder","On request","ST",1,"LP",1,"8PQ91510AA25"]
["8PQ9154-0AA87","partition","On request","ST",1,"LP",1,"8PQ91540AA87"]
["8PQ9155-7AA02","bracket","On request","ST",1,"LP",1,"8PQ91557AA02"]
["8PQ9157-1AA42","holder 25x25 w08","On request","ST",1,"LP",1,"8PQ91571AA42"]
["8PQ9158-4AA51","Latch height 78","On request","ST",1,"LP",1,"8PQ91584AA51"]
["8PQ9163-0AA26","mounting plate","On request","ST",1,"LP",1,"8PQ91630AA26"]
["8PQ9203-2AA51","Socket 63 A","On request","ST",1,"LP",50,"8PQ92032AA51"]
["8PQ9400-0BA76","SIVACON S4 IP55 Sealing 10x4mm L=5,5m 1 Pack=10 Pieces",135,"ST",1,"LP",1,"8PQ94000BA76"]
["8PQ9700-0AA46","SIVACON S8 FRANCHISE TAU 3","On request","ST",1,"LP",1,"8PQ97000AA46"]
["8UC7120-3BB","8UC7 handle with masking frame Red handle masking frame yellow Spare part for 8UC7121-3BB10",55.7,"ST",1,"LP",1,"8UC71203BB"]
["8UD1171-1AD25","Door-coupling rotary operating mechanism Emergency switching off with tolerance compensation Size 75x 75, Shaft 6x6, 300 mm, 0-1, Complete unit Handle size 45 mm Accessory for 3KD0 size 01 and 02",36.300000000000004,"ST",1,"LP",1,"8UD11711AD25"]
["8US1211-4TR00","busbar adapter 60 mm SYS UL 508 Busbar system 60 mm Bar thickness: 5/10 mm/TT profile UL rating 100A/600V Can be used in spring circuits IEC rating 100 A/690 V for SIRIUS circuit breaker for SIRIUS Size S3 for cable outlet top Cable welded 150Β° 153mm Adapter length 200 mm Adapter width 72 mm",128,"ST",1,"LP",1,"8US12114TR00"]
["8US1922-1AC00-0AA1","Busbar system, accessories Busbar center-to-center spacing 60 mm End cover for busbar holder for 8US1923-3AA01 3-pole or for 8US1923-2AA01 3-pole",10.6,"ST",1,"LP",1,"8US19221AC000AA1"]
["8WA1011-1BP11","Through-type terminal thermoplast Screw terminal on both sides Single terminal blue 25 mm, Sz. 70",17.600000000000001,"ST",1,"LP",10,"8WA10111BP11"]
["8WA1221","Through-type terminal thermoplast Soldered connection on both sides 5.5mm, Size 1.5",4.7300000000000004,"ST",1,"LP",50,"8WA1221"]
["8WA8347-2AE","inscription label, front, with L3, horizontal, terminal width: 5 mm, H: 7 mm, white",9.6300000000000008,"ST",100,"LP",136,"8WA83472AE"]
["8WC5055","Flat copper rod 30x 5 mm approx. 2 meter long zinc plated",201,"ST",1,"LP",3,"8WC5055"]
["8WD4308-0ED","pipe individually, Length 1000 mm, accessory for signaling columns, with diameters 50 mm and 70 mm",82,"ST",1,"CP",1,"8WD43080ED"]
["8WD4420-0CD","Single-flash light element, w. built-in electronic flash, yellow, 24 V DC, Diameter 70 mm",154,"ST",1,"CP",1,"8WD44200CD"]
["8WH1000-1MG88","Fuse terminal LED 110-250 V with screw terminal Terminal size 4.0 mm2 Terminal width 6.2 mm Color black fuse 5x 20 mm",10.199999999999999,"ST",1,"LP",50,"8WH10001MG88"]
["8WH2000-0CK07","Protective conductor terminal with spring-loaded connection, Cross-section: 1.5-16 mm2, Width: 12mm, Color: green-yellow",5.03,"ST",1,"LP",25,"8WH20000CK07"]
["8WH2020-0AG01","Two-tier terminals with spring-loaded connection, Cross-section: 0.5-4 mm2, Width: 6.2mm, Color: blue",2.14,"ST",1,"LP",50,"8WH20200AG01"]
["8WH8111-0AA05","Labeling plates 3.5 mm flat, unprinted",5.69,"ST",100,"LP",100,"8WH81110AA05"]
["8WH8121-1AB75","Labeling plate, flat, with 71-80, vertical, Terminal width: 4.2 mm, H: 6.4 mm, white",7.1,"ST",100,"LP",100,"8WH81211AB75"]
["8WH8140-2AC05","Labeling plate, front, with 91-100, horizontal, Terminal width: 5.2 mm, H: 6.4 mm, white",7.53,"ST",100,"LP",100,"8WH81402AC05"]
["8WH9003-1VA00","cover for two-tier terminals with spring-loaded connection Cross-section: 4 mm2, Width: 2.2mm, Color: gray",54.7,"ST",100,"LP",50,"8WH90031VA00"]
["8WH9063-5AA06","inscription label, with lightning symbol, vertical, terminal width: 6.2 mm, yellow",25.3,"ST",100,"LP",50,"8WH90635AA06"]
["8WH9150-1CA00","terminal strip markers f. 8WH9150-0CA00, facility f. labeling, size 10",0.65,"ST",1,"LP",100,"8WH91501CA00"]
["LZS:PT5A5L24","Plug-in relay complete unit 4 W, 24 V DC LED module red Standard plug-in socket screw terminal 3.5 mm pinning",16.3,"ST",1,"CP",5,"LZS:PT5A5L24"]
["SWB:55668","spare part for 3AH, 3AK, 3AE aux. contactor AC 50/60Hz 125V","On Request","ST",1,"LP",1,"SWB:55668"]
["SWB:PTD0081730750","Torsion Spring","On Request","ST",1,"LP",1,"SWB:PTD0081730750"]
["US2:A02MN64","Breaker MD-RD 480V AC 2AUX Software ACC","On request","ST",1,"LP",1,"US2:A02MN64"]
["US2:CED62M125","Breaker ED 2P 125A 600V 100kA 50C LD LUG","On request","ST",1,"LP",1,"US2:CED62M125"]
["US2:CFD63B200L","Breaker FD 3P 200A 600V 100kA LUGS","On request","ST",1,"LP",1,"US2:CFD63B200L"]
["US2:CLD63B600","Breaker LD 3P 600A 600V 100kA NL","On request","ST",1,"LP",1,"US2:CLD63B600"]
["US2:CQD6345","Breaker CQD 3P 45A 347VAC 14kA DIN CSA","On request","ST",1,"LP",1,"US2:CQD6345"]
["US2:CQDST600AASWC","Molded case circuit breaker Accessory for BQD, CQD, NGG, HGG, LGG, NGB, HGB, LGB Shunt release and Auxiliary switch block combination Voltage: 600 V AC Version for West Chicago","On request","ST",1,"LP",1,"US2:CQDST600AASWC"]
["US2:ED23M040","Breaker ED 3P 40A 240VAC 10kA 50C LD LUG","On request","ST",1,"LP",1,"US2:ED23M040"]
["US2:ED42B040","Breaker ED 2P 40A 480V AC 18kA LD LUG","On request","ST",1,"LP",1,"US2:ED42B040"]
["US2:ED61B020","Breaker ED 1P 20A 347V 30kA LD LUG CSA","On request","ST",1,"LP",1,"US2:ED61B020"]
["US2:EM6B010MS2L","Breaker MINING 10A 600V 18kA MAG","On request","ST",1,"LP",1,"US2:EM6B010MS2L"]
["US2:FD63F250","Breaker FD 3P 250A 600V 22kA FR","On request","ST",1,"LP",1,"US2:FD63F250"]
["US2:FDS20R","Breaker MC FXD DEPTH Flange Software OPER RT","On request","ST",1,"LP",1,"US2:FDS20R"]
["US2:FXD63M150L","Breaker FD 3P 150A 600V 22kA 50C FX LUGS","On request","ST",1,"LP",1,"US2:FXD63M150L"]
["US2:HEB3B125B","Breaker HEB 3P 125A 480V 65kA LOAD LUGS","On request","ST",1,"LP",1,"US2:HEB3B125B"]
["US2:HED42M090","Breaker ED 2P 90A 480V 42kA 50C LD LUG CALIB 50C","On request","ST",1,"LP",1,"US2:HED42M090"]
["US2:HED43B125NAV","Breaker HED4 3P 125A 600V 18kA LD LG NAV","On request","ST",1,"LP",1,"US2:HED43B125NAV"]
["US2:HEM3M070L","Breaker EG 3P 70A MCP MID MAG LUGS","On request","ST",1,"LP",1,"US2:HEM3M070L"]
["US2:HGB2K045B","Circuit Breaker HGB HGB2K045B Certification acc. UL489 2 Pole; Rated current lN=45A max. voltage 600Y/347V AC NEMA rating 35kA @ 480V NEMA rating 22kA @ 600Y/347V load lugs included","On request","ST",1,"LP",1,"US2:HGB2K045B"]
["US2:HHED63B050","Breaker ED 3P 50A 600V 18kA LD LUG","On request","ST",1,"LP",1,"US2:HHED63B050"]
["US2:HJXD63B225L","Breaker JD 3P 225A 600V 35kA FXD LUGS","On request","ST",1,"LP",1,"US2:HJXD63B225L"]
["US2:HMXD63B700H","Breaker MD 3P 700A 600V 50kA FXD 100","On request","ST",1,"LP",1,"US2:HMXD63B700H"]
["US2:JMKF400","Breaker MINING 400A 1kV 14kA FR","On request","ST",1,"LP",1,"US2:JMKF400"]
["US2:JXD23B200L","Breaker JD 3P 200A 240V 65kA FX LUGS","On request","ST",1,"LP",1,"US2:JXD23B200L"]
["US2:LGB3K040B","Circuit Breaker LGB LGB3K040B Certification acc. UL489 3 Pole; Rated current lN=40A max. voltage 600Y/347V AC NEMA rating 65kA @ 480V NEMA rating 25kA @ 600Y/347V load lugs included","On request","ST",1,"LP",1,"US2:LGB3K040B"]
["US2:LMKT600MC3","Breaker MINING 600A 1kV 14kA MAG TU","On request","ST",1,"LP",1,"US2:LMKT600MC3"]
["US2:LXD63H600L","Breaker LD 3P 600A 35kA FX HI ETI LUGS","On request","ST",1,"LP",1,"US2:LXD63H600L"]
["US2:MM9301","Breaker MINING 1600A Mounting Base ACC","On request","ST",1,"LP",1,"US2:MM9301"]
["US2:N06SMDA","Breaker SMD 600A NEUT Transformator","On request","ST",1,"LP",1,"US2:N06SMDA"]
["US2:NEB2B100B","Breaker NEB 2P 90A 480V 35kA LOAD LUGS","On request","ST",1,"LP",1,"US2:NEB2B100B"]
["US2:NGB1B045V","Circuit Breaker NGB NGB1B045V Certification acc. UL489 1 Pole; Rated current lN=45A max. voltage 347V AC NEMA rating 25kA @ 277V NEMA rating 14kA @ 347V load lugs included bulk pack","On request","ST",1,"LP",1,"US2:NGB1B045V"]
["US2:NGB2B125V","Circuit Breaker NGB NGB2B125V Certification acc. UL489 2 Pole; Rated current lN=125A max. voltage 600Y/347V AC NEMA rating 25kA @ 480Y/277V NEMA rating 14kA @ 600Y/347V load lugs included bulk pack","On request","ST",1,"LP",1,"US2:NGB2B125V"]
["US2:NGB3B100V","Circuit Breaker NGB NGB3B100V Certification acc. UL489 3 Pole; Rated current lN=100A max. voltage 600Y/347V AC NEMA rating 25kA @ 480Y/277V NEMA rating 14kA @ 600Y/347V load lugs included bulk pack","On request","ST",1,"LP",1,"US2:NGB3B100V"]
["US2:NGB3K080B","Circuit Breaker NGB NGB3K080B Certification acc. UL489 3 Pole; Rated current lN=80A max. voltage 600Y/347V AC NEMA rating 25kA @ 480V NEMA rating 14kA @ 600Y/347V load lugs included","On request","ST",1,"LP",1,"US2:NGB3K080B"]
["US2:NGG3B060","Circuit Breaker NGG NGG3B060 Certification acc. UL489 3 Pole; Rated current lN=60A max. voltage 600Y/347V AC NEMA rating 25kA @ 480V NEMA rating 14kA @ 600Y/347V no lugs","On request","ST",1,"LP",1,"US2:NGG3B060"]
["US2:QJ23B08001S01","MCCB 3P 80A 10K W/Shunt Trip and AUX",8036,"ST",1,"LP",1,"US2:QJ23B08001S01"]
["US2:QJH23B175","Breaker QJ 3P 175A 240V 22kA",7257,"ST",1,"LP",1,"US2:QJH23B175"]
["US2:S01JLD62A","Breaker JD/LD/LMD 120VAC ST/AUX Software","On request","ST",1,"LP",1,"US2:S01JLD62A"]
["US2:SCLD69600G","Breaker SLD 3P 600A 600V 100kA LIG",95391,"ST",1,"LP",1,"US2:SCLD69600G"]
["US2:SCMD69700ANGTH","Breaker SMD 3P 700A 600V 65kA LSIG 100",128688,"ST",1,"LP",1,"US2:SCMD69700ANGTH"]
["US2:SCND6B100LSIH","Circuit Breaker SENTRON Type SCND SCND6B100LSIH Certification acc. UL489 3 Pole Rated current lN=1000A NEMA rating 65 kA @ 600V NEMA rating 100KA @ 480V 100% Rated electronic trip unit, LSIH","On request","ST",1,"LP",1,"US2:SCND6B100LSIH"]
["US2:SHLD6B400LSI","Circuit Breaker SENTRON Type SHLD SHLD6B400LSI Certification acc. UL489 3 Pole Rated current lN=400A NEMA rating 35 kA @ 600V NEMA rating 65KA @ 480V 80% Rated electronic trip unit, LSI","On request","ST",1,"LP",1,"US2:SHLD6B400LSI"]
["US2:SHND69120AGH","Breaker SND 3P 1200A 600V 50kA LIG 100",99441,"ST",1,"LP",1,"US2:SHND69120AGH"]
["US2:SHPD6A140LIG","Circuit Breaker SENTRON Type SHPD SHPD6A140LIG Certification acc. UL489 3 Pole Rated current lN=1400A NEMA rating 50 kA @ 600V NEMA rating 65KA @ 480V 80% Rated electronic trip unit, LIG","On request","ST",1,"LP",1,"US2:SHPD6A140LIG"]
["US2:SJD6A300LIGH","Circuit Breaker SENTRON Type SJD SJD6A300LIGH Certification acc. UL489 3 Pole Rated current lN=300A NEMA rating 25 kA @ 600V NEMA rating 35KA @ 480V 100% Rated electronic trip unit, LIGH","On request","ST",1,"LP",1,"US2:SJD6A300LIGH"]
["US2:SMD6A800LSIGH","Circuit Breaker SENTRON Type SMD SMD6A800LSIGH Certification acc. UL489 3 Pole Rated current lN=800A NEMA rating 25 kA @ 600V NEMA rating 50KA @ 480V 100% Rated electronic trip unit, LSIGH","On request","ST",1,"LP",1,"US2:SMD6A800LSIGH"]
["US2:SND6B800LIGH","Circuit Breaker SENTRON Type SND SND6B800LIGH Certification acc. UL489 3 Pole Rated current lN=800A NEMA rating 25 kA @ 600V NEMA rating 50KA @ 480V 100% Rated electronic trip unit, LIGH","On request","ST",1,"LP",1,"US2:SND6B800LIGH"]
["US2:U01ED60","Breaker ED 120VAC UV TRP","On request","ST",1,"LP",1,"US2:U01ED60"]
["US2:U11MN64AA","Breaker MN/ND/PD/RD 125V DC UV TRP/2AUX","On request","ST",1,"LP",1,"US2:U11MN64AA"]
["XPT:8PT1015","Door IP54 H2200 W1000 right",1016,"ST",1,"LP",1,"XPT:8PT1015"]
["XPT:8PT10708","Compartment door W800 H2175 right IP42",1178,"ST",1,"LP",1,"XPT:8PT10708"]
["XPT:8PT11294","Support",70.199999999999989,"ST",1,"LP",5,"XPT:8PT11294"]
["XPT:8PT12540","Support 3",41.1,"ST",1,"LP",10,"XPT:8PT12540"]
["XPT:8PT13005","Compartment door W800 H625 left",387,"ST",1,"LP",1,"XPT:8PT13005"]
["XPT:8PT13439","Holder",70.099999999999994,"ST",1,"LP",10,"XPT:8PT13439"]
["XPT:8PT13911","Vertical busbar holder BC W",12.6,"ST",1,"LP",50,"XPT:8PT13911"]
["XPT:8PT14684","Section door IP54 H625 B06 right 3",628,"ST",1,"LP",1,"XPT:8PT14684"]
["XPT:8PT14963","Fixed cover 2x VL160/250 3/4-pol.",102,"ST",1,"LP",5,"XPT:8PT14963"]
["XPT:8PT15408","Compartment bottom 3WL B600",83.1,"ST",1,"LP",5,"XPT:8PT15408"]
["XPT:8PT16283","Mounting plate 275x 850 CCS",66.899999999999991,"ST",1,"LP",5,"XPT:8PT16283"]
["XPT:8PT17080","Section door 20X08 IP40 right",932,"ST",1,"LP",1,"XPT:8PT17080"]
["XPT:8PT17400","Frame profile corner cubicle H400",61,"ST",1,"LP",2,"XPT:8PT17400"]
["XPT:8PT17795","Support ALPHA B850",46.2,"ST",1,"LP",10,"XPT:8PT17795"]
["XPT:8PT20179","Partition F connecting bar F L,",19.200000000000003,"ST",1,"LP",20,"XPT:8PT20179"]
["XPT:8PT20988","Partition 800 horiz. left",76.5,"ST",1,"LP",5,"XPT:8PT20988"]
["XPT:8PT21779","Mounting bracket 2 bar M",80.099999999999994,"ST",1,"LP",5,"XPT:8PT21779"]
["XPT:8PT22047","Mounting plate 3VL400 4-pole Socket",72.5,"ST",1,"LP",5,"XPT:8PT22047"]
["XPT:8PT22634","Mounting plate 600",80.5,"ST",1,"LP",5,"XPT:8PT22634"]
["XPT:8PT23033","Cover 2 3NP44",35.6,"ST",1,"LP",10,"XPT:8PT23033"]
["XPT:8PT23670","Cover 700",31.900000000000002,"ST",1,"LP",10,"XPT:8PT23670"]
["XPT:8PT24420","Base COMPARTMENT Cover H225 W600 IP4",140,"ST",1,"LP",1,"XPT:8PT24420"]
["XPT:8PT24874","Housing 200",31.900000000000002,"ST",1,"LP",10,"XPT:8PT24874"]
["XPT:8PT263","Frame rear panel 800 top",51.4,"ST",1,"LP",10,"XPT:8PT263"]
["XPT:8PT30831","SIVACON connection LXA0541-FA3A I=1600A, U=690 V, full pen Connection of rail to distributor top",2042,"ST",1,"LP",1,"XPT:8PT30831"]
["XPT:8PT3440","Brace right OFW",106,"ST",1,"LP",5,"XPT:8PT3440"]
["XPT:8PT3809","Touch protection bar 3W",160,"ST",1,"LP",5,"XPT:8PT3809"]
["XPT:8PT395","Compartment door top W600 LT1 RI",209,"ST",1,"LP",1,"XPT:8PT395"]
["XPT:8PT50468","SIVACON 8PT switchboard Copper surcharge","On Request","ST",1,"LP",1,"XPT:8PT50468"]
["XPT:8PT5233","Door 20X04 LI non-ventilated IP40",486,"ST",1,"LP",1,"XPT:8PT5233"]
["XPT:8PT544","Support for HSS UV",121,"ST",1,"LP",5,"XPT:8PT544"]
["XPT:8PT600","Transformer bar holder 800",84.6,"ST",1,"LP",5,"XPT:8PT600"]
["XPT:8PT6539","standard",8.0399999999999991,"ST",1,"LP",50,"XPT:8PT6539"]
["XPT:8PT7475","Cover 600mm 162.5/282 8UC63/66",136,"ST",1,"LP",5,"XPT:8PT7475"]
["XPT:8PT7693","Vertical strut 206",20.400000000000002,"ST",1,"LP",20,"XPT:8PT7693"]
["XPT:8PT9667","Latch plate",617,"ST",100,"LP",100,"XPT:8PT9667"]
["6AG1040-1LA00-2AA0","SIPLUS S120 Control Unit CU310-2 DP -20...+55Β°C with conformal coating based on 6SL3040-1LA00-0AA0 . with PROFIBUS interface without CompactFlash card",1336,"ST",1,"SIMATIC",1,"6AG10401LA002AA0"]
["6AG1134-6TD00-2CA1","SIPLUS ET 200SP 4xAI 2-wire 4-20 mA HART -40...+60 Β°C start up 30 Β°C with conformal coating based on 6ES7134-6TD00-0CA1 . analog HART input module, AI 4XI 2-wire HART high feature suitable for BU type A0, A1, color code CC03, channel diagnostics, 16-bit, +/-0.3%",860,"ST",1,"SIMATIC",1,"6AG11346TD002CA1"]
["6AG1212-1AE40-2XB0","SIPLUS S7-1200 CPU 1212C DC/DC/DC -40...+70Β°C with conformal coating based on 6ES7212-1AE40-0XB0 . compact \"CPU, DC/DC/DC, onboard I/O: \"\"8\" \"DI 24 V DC;\"\" \"\"6 DO 24 V DC;\"\" 2\" AI 0-10 V DC, Power supply: 20.4-28.8V DC, Program/data memory 75 KB",470,"ST",1,"S7-1200",1,"6AG12121AE402XB0"]
["6AG1331-6SB00-7AY0","SIPLUS LOGO! Power 24V 1,3A for medial stress -40...+70Β°C start up at -25Β°C based on 6EP3331-6SB00-0AY0 . stabilized power supply input: AC 100-240 V output: DC 24 V / 1,3 A",210,"ST",1,"LOGO!",1,"6AG13316SB007AY0"]
["6AG1433-2BA20-7AA0","SIPLUS PS PSU300S 5A -25 ... +70Β°C with conformal coating based on 6EP1433-2BA20. STABILIZED POWER SUPPLY INPUT: 3 400-500 V 3AC OUTPUT: 24 V DC/5 A",415,"ST",1,"SIMATIC",1,"6AG14332BA207AA0"]
["6AG1803-4BA00-7AA0","SIPLUS NET TIM 4R-IE DNP3 -25...+70Β°C with conformal coating based on 6NH7803-4BA00-0AA0. TIM 4R-IE DNP3 communication module for \"SIMATIC S7-300, \"\"S7-400, PC;\" \"with two\"\" RS232/RS485\" interfaces for DNP3 communication via classic WANs and two RJ45 interfaces for DNP3 communication via IP- based networks (WAN or LAN)",5067,"ST",1,"SIMATIC",1,"6AG18034BA007AA0"]
["6AG2623-0AA00-4AA0","SIPLUS PN/J1939 LINK TX RAIL -40...+70Β°C TX with 85Β°C for 10min with Conformal Coating based on 6BK1623-0AA00-0AA0 . gateway from Profinet to J1939 networks, IP20",1011,"ST",1,"SIMATIC",1,"6AG26230AA004AA0"]
["6AV2103-2AD00-0UC0","SIMATIC WinCC Professional V17 UCL (TIA Portal) Powerpack WinCC Advanced V17 -> WinCC Professional 512 PowerTags V17, for one installation; engineering software; software and documentation on DVD; master license on CD; UCL agreement required",239,"ST",1,"SIMATIC",1,"6AV21032AD000UC0"]
["6AV2104-0BA00-0AR0","EPL Maintenance for SIMATIC WinCC Runtime Advanced 128 Power Tags; (EPL=Enterprise License) Payment for maintenance of a Royalty for 12 months, only valid in connection with Enterprise License contract, requires EPL Master",92,"ST",1,"SIMATIC",1,"6AV21040BA000AR0"]
["6AV2105-3DD07-0AE0","SIMATIC WinCC RT Professional, 512 PowerTags V17, upgrade V11..V16 -> V17, runtime software in TIA Portal, single license, SW and documentation on DVD, license key on USB flash drive, class A, 5 languages (de,en,fr,es,it), please observe product release: support.industry.siemens.com entry ID: 109771219 ******************************* content: set (2x DVD + 1x USB)",1699,"ST",1,"SIMATIC",1,"6AV21053DD070AE0"]
["6AV2107-0RA00-0BQ0","EPL Royalty for SIMATIC WinCC Audit for Runtime Advanced; only valid in connection with Enterprise License contract, requires EPL Master",812,"ST",1,"SIMATIC",1,"6AV21070RA000BQ0"]
["6AV2123-2JB03-0AX0","SIMATIC HMI, KTP900 Basic, Basic Panel, Key/touch operation, 9\" TFT display, 65536 colors, PROFINET interface, configurable from WinCC Basic V13/ STEP 7 Basic V13, contains open-source software, which is provided free of charge see enclosed CD",1158,"ST",1,"SIMATIC",1,"6AV21232JB030AX0"]
["6AV2124-2DC01-0AX0","SIMATIC HMI KTP400 Comfort, Comfort Panel, key/touch operation, 4\" widescreen TFT display, 16 million colors, PROFINET interface, MPI/PROFIBUS DP interface, 4 MB configuration memory, Windows CE 6.0, configurable from WinCC Comfort V11",713,"ST",1,"SIMATIC",1,"6AV21242DC010AX0"]
["6AV2153-0XB60-0LB5","SIMATIC WinCC Unified V17 PC Engineering Powerpack Professional max. -> PC max. PowerTags (without change of version)V16..V17; engineering software in the TIA Portal; Floating License; without software and documentation; license key for download; class A; ******************************* goods recipient email address required for delivery",2332,"ST",1,"SIMATIC",1,"6AV21530XB600LB5"]
["6AV2154-2FB01-7LA0","SIMATIC WinCC Unified V17 PC Runtime 10k PowerTags, runtime software in in TIA Portal; Single License; with software documentation and license key for download; class A; 5 languages: de,en,fr,es,it; please observe product release: support.industry.siemens.com entry ID: 109792168 ******************************* goods recipient email address required for delivery",5300,"ST",1,"SIMATIC",1,"6AV21542FB017LA0"]
["6AV2157-2CM00-0LB0","SIMATIC WinCC Unified Client, 10 Monitor Clients, option for WinCC Unified, runtime software, Single License without software and documentation; license key for download; class A; ******************************* goods recipient email address required for delivery",4548,"ST",1,"SIMATIC",1,"6AV21572CM000LB0"]
["6AV6371-1CB07-0AQ0","EPL Royalty for WinCC V7, User Archives option. only valid in connection with Enterprise License agreement, requires EPL Master",841,"ST",1,"SIMATIC",1,"6AV63711CB070AQ0"]
["6AV6371-2BM07-4AJ0","WinCC Powerpack RT 2048/8192 for WinCC V7.4, Runtime license without version change from 2048 to 8192 PowerTags, single license, license key download ******************************* Email address required for delivery",932,"ST",1,"SIMATIC",1,"6AV63712BM074AJ0"]
["6AV6372-2BJ17-5BA1","Sequence Execution System, Extension 5 Units Upgrade, for SIMATIC WinCC V7.5 SP1, Runtime software, single license, count relevant, License key on USB flash drive ******************************* Content: 1x USB",426,"ST",1,"SIMATIC",1,"6AV63722BJ175BA1"]
["6AV6372-2DF47-0AX0","SIMATIC Energy Manager PRO Energy forecast and planning; Engineering/Runtime software; Single License; license key on USB stick; without software and documentation ******************************* Content: 1x USB",6617,"ST",1,"SIMATIC",1,"6AV63722DF470AX0"]
["6AV6381-2BS07-4AH0","WinCC system software V7.4 SP1, RC 8192 (8192 PowerTags), runtime/configuration software, Floating License, software and license key download class A, 5 languages (de,en,fr,es,it), executable under Windows 7 Professional/Enterprise/Ultimat e +SP1 (32-bit)/ 7 Professional/Enterprise/Ultimat e +SP1 (64-bit)/ 8.1 Professional/Enterprise (32-bit)/ 8.1 Professional/Enterprise (64-bit)/ 10 Professional/Enterprise (64-bit)/ Server 2008 R2+SP1 (64-bit)/ Server 2012 R2 (64-bit)/ Server 2016 (64-bit) ****************************(*)",9958,"ST",1,"SIMATIC",1,"6AV63812BS074AH0"]
["6AV6381-2CB07-4AK3","SIMATIC WinCC RC client upgrade from V7.X to V7.4 SP1, for WinCC RC Clients without RC 128, runtime/configuration software, single license, software and license key download ******************************* Email address required for delivery",974,"ST",1,"SIMATIC",1,"6AV63812CB074AK3"]
["6AV6613-1BA51-3CA0","WinCC flexible 2008 Runtime 128 PowerTags runtime software, single license SW and documentation on CD, license key on USB flash drive executable in Windows 7 Prof/Ultimate/Enterprise(32/64) Windows 10 Pro/Enterprise (64) ******************************* Content: Set (1x DVD + 1x USB)",749,"ST",1,"SIMATIC",1,"6AV66131BA513CA0"]
["6AV6646-1BA15-0AA0","SIMATIC ITC1500 V3, Industrial Thin Client, 15\" widescreen TFT display, capacitive touch sensor, Supported protocols: RDP, VNC, SMARTSERVER HTML5 et. al., Standard Design, panel mount",1676,"ST",1,"SIMATIC",1,"6AV66461BA150AA0"]
["6AV7674-1LB15-0AA0","Grip handles for HMI PRO devices, universally adjustable from 24\", RAL9006 (silver)",364,"ST",1,"SIMATIC",1,"6AV76741LB150AA0"]
["6AV7863-5MA15-2AA0","SIMATIC IFP1500 V2 PRO, 15 multi-touch display (16:9) with 1920x1080 pixel resolution, PRO variant support arm, for 24 V DC, DisplayPort, can be placed up to 100 m away HDBaseT, USB on the rear side, standard design",1730,"ST",1,"SIMATIC",1,"6AV78635MA152AA0"]
["6BK1700-2GA00-0AA0","spare part SIPLUS HCS4300 fan for HCS POM4320",84.399999999999991,"ST",1,"SIMATIC",1,"6BK17002GA000AA0"]
["6ED1057-1DA00-0BA0","LOGO! TD mounting accessories Spare parts for LOGO! TD",11.7,"ST",1,"LOGO!",1,"6ED10571DA000BA0"]
["6ES7193-6BP00-0DA0","SIMATIC ET 200SP, BaseUnit BU15-P16+A0+2D, BU type A0, push-in terminals, without aux. terminals, new load group, WxH: 15x 117 mm",26,"ST",1,"SIMATIC",1,"6ES71936BP000DA0"]
["6ES7193-6CP86-2AC0","SIMATIC ET 200SP, 10 color-coded labels Color code CC86, for 2 AUX terminals, for BU type C0, with push-in terminals",11.799999999999999,"PAK",1,"SIMATIC",1,"6ES71936CP862AC0"]
["6ES7195-1GC00-0XA0","SIMATIC DP, mounting rail for ET 200M, 2000 mm long, for holding bus modules for removal and insertion function",203,"ST",1,"SIMATIC",1,"6ES71951GC000XA0"]
["6ES7313-5BG04-0AB0","SIMATIC S7-300, CPU 313C, Compact CPU with MPI, 24 DI/16 DO, 4 AI, 2 AO, 1 Pt100, 3 high-speed counters (30 kHz), Integr. power supply 24 V DC, work memory 128 KB, Front connector (2x 40-pole) and Micro Memory Card required",1183,"ST",1,"SIMATIC",1,"6ES73135BG040AB0"]
["6ES7360-3AA01-0AA0","SIMATIC S7-300, Connection IM 360 in central rack for connection of max. 3 expansion racks, with C-bus",250,"ST",1,"SIMATIC",1,"6ES73603AA010AA0"]
["6ES7516-3AN02-0AB0","SIMATIC S7-1500, CPU 1516-3 PN/DP, central processing unit with 1 MB work memory for program and 5 MB for data, 1st interface: PROFINET IRT with 2-port switch, 2nd interface: PROFINET RT, 3rd interface: PROFIBUS, 10 ns bit performance, SIMATIC Memory Card required",3825,"ST",1,"SIMATIC",1,"6ES75163AN020AB0"]
["6ES7590-1AJ30-0AA0","SIMATIC S7-1500, mounting rail 830 mm (approx. 32.7 inch); incl. grounding screw, integrated DIN rail for mounting of incidentals such as terminals, automatic circuit breakers and relays",47.5,"ST",1,"SIMATIC",1,"6ES75901AJ300AA0"]
["6ES7677-2SB42-0GL0","SIMATIC ET 200SP Open Controller, CPU 1515SP PC2 F + HMI 512PT, 8 GB RAM, 128 GB CFast with Windows 10 IoT Enterprise 64-bit, S7-1500 Failsafe Software Controller CPU 1505SP F and WinCC Runtime Advanced pre-installed, with 512 PowerTags license; Interfaces: 1x Slot CFast, 1x slot SD/MMC, 1x connection for ET 200SP bus Adapter PROFINET, 1x 10/100/1000 Mbit/s Ethernet, 2x USB 3.0, 2x USB 2.0, 1x display port, Documentation on CFast Restore image on CFast",4004,"ST",1,"SIMATIC",1,"6ES76772SB420GL0"]
["6ES7822-1AA00-0YM5","SIMATIC STEP 7 Professional Software Update Service (SUS) Compact for STEP 7 TIA Portal; for multiple orders on one position, these deliveries are grouped. Minimum order quantity: 3 units within the framework of this contract, you will receive for one year all up-to-date software versions. the contract is extended automatically by 1 year if it is not canceled 3 months prior to expiration. Period of delivery and service: 1 year from date of invoice. Requirement for conclusion: current version of the software",441,"ST",1,"SIMATIC",1,"6ES78221AA000YM5"]
["6ES7823-1AE07-0YA5","TIA Portal Multiuser Engineering V17 Floating License download; option for engineering software in TIA Portal; software and documentation in STEP 7 / WinCC download; license key for download; class A; 9 languages: de,en,zh included, fr,sp,it,ru,jp,kr as download; executable in Windows 10, Windows Server 2016/2019; ******************************* Email address required for delivery",541,"ST",1,"SIMATIC",1,"6ES78231AE070YA5"]
["6ES7860-4AA01-0YX1","SIMATIC S7, PID self tuner V5.1 single license for 1 installation R-SW, without SW and without documentation, Class A, 2 languages (de, en), Reference HW: S7-300/-400, C7",79.199999999999989,"ST",1,"SIMATIC",1,"6ES78604AA010YX1"]
["6GF6710-2BC","PS 2 membrane keyboard INT, with touch pad, desktop keyboard for devices with corresponding interface Further information, Quantity and content: see technical data",817,"ST",1,"SIMATIC",1,"6GF67102BC"]
["7KG6106-2EN24-0B","Simeas transmitter (G) MUU for alternating voltage in the enclosure, for snapping on standard mounting rail Rated frequency 50 Hz Input voltage 100 V AC Output signal DC 4 to 20 mA (live zero) Auxiliary power 88-264 V DC Measuring range linear 0 up to UEN",718,"ST",1,"SIMATIC",1,"7KG61062EN240B"]
["7KG6131-1BM14","Simeas T transmitter for direct current, Direct voltage and isolation amplifier Input voltage: 150 mV to 150 mV DC Output signal: 10 V to 10 V DC Zero position: Input: 0 mA, V=output: 0 mA, V Auxiliary power 88 V to 284 V DC",995,"ST",1,"SIMATIC",1,"7KG61311BM14"]
["A5E43790667","SIMATIC HMI, TP2200 Comfort 2, neutral, Purch, Basic: 6AV2124-0XC02-0AX1 for internal use only",4868,"ST",1,"SIMATIC",1,"A5E43790667"]
["6GF3540-0CD10","SIMATIC MV540 S optical reader Resolution: 800 x 600 pixels, Function: 1D/2D code reading; Image field and distance: variable, (ABH lens object); PoE; IP67 with 6GF3540-8AC11; Delivery: Reader and SD card adapter;",2184,"ST",1,"SIMATIC",1,"6GF35400CD10"]
["6GK1571-0BA00-0AA0","PC adapter USB A2 USB adapter (USB V2.0) for connection of a PG/PC or notebook to SIMATIC S7 via PROFIBUS or MPI contain USB cable 5 m, MPI cable 0.3 m can be used under Windows XP/Vista/ Windows 7 32/64-bit and higher",431,"ST",1,"SIMATIC",1,"6GK15710BA000AA0"]
["6GK1716-0HB15-0AA0","HARDNET-IE S7 REDCONNECT V15 incl. OPC server and IE-S7 SW for fail-safe S7 comm.; Floating License; R-SW, SW + electr. manual on DVD, license key on USB flash drive, Class A 2 languages (de, en); for Windows 7 SP1 Prof./Ult. (64 bit); WindowsΒ® Server 2008 R2 SP1, WindowsΒ® Server 2012 R2; WindowsΒ® 10 Pro / Enterprise (64 bit), from Version 1607; WindowsΒ® Server 2016 for max. 4 CP 1613 A2, CP 1623, CP 1628",2069,"ST",1,"SIMATIC",1,"6GK17160HB150AA0"]
["6GK1901-0DM40-2AA5","IE M12 panel feedthrough 4x 2 Control cabinet bushing for transition from M12 connection system (X-coded, IP65/67) to RJ45 connection system IP20 1 pack = 1 unit",352,"ST",1,"SIMATIC",1,"6GK19010DM402AA5"]
["6GK5201-3BH00-2BA3","SCALANCE X201-3PIRT managed IE IRT switch, 1x 10/100 Mbit/s RJ45 ports, 3x 100 Mbit/s POF SC RJ ports, Error signaling contact with set button, Redundant power supply, PROFINET IO device, network management, Redundancy Manager integrated, incl. electron. manual on CD-ROM, C-plug optional",1218,"ST",1,"SIMATIC",1,"6GK52013BH002BA3"]
["6GK5324-4QG10-1AR2","SCALANCE XR324-4M PoE; Managed IE switch, 19\" rack; 8x 10/100/1000 Mbit/s for RJ45 ports electrical with PoE, 8x 10/100/1000 Mbit/s for RJ45 ports electrical without PoE; 4x 10/100/1000 Mbit/s 2-port media modules, electrical or optical; LED diagnostics; error signaling Contact; Select/set pushbutton, PROFINET IO device, Power supply 24 V DC; Ports in the front",4074,"ST",1,"SIMATIC",1,"6GK53244QG101AR2"]
["6GK5778-1GY00-0TA0","IWLAN access point, SCALANCE W778-1 M12 EEC, 1 radio, 2 N-CON antenna port, iFeatures support via key plug, IEEE 802.11a/b/g/h/n, 2.4/5 GHz, gross data rate 300 Mbit/s, 2x M12 max. 100 Mbit/s, PoE integrated 2-port switch, redundant 24 V DC, M12 A-coded IP65, -30... 70 Β°C, plug slot WPA2/802.11i/e,conformal coating EN 50155, EN 45545, observe national approvals! CERT ID: MSN65-W1-M12-E2 Scope of delivery: Manuals on CD-ROM, English/German; M12 sealing caps, for operation outside of USA/Israel",1376,"ST",1,"SIMATIC",1,"6GK57781GY000TA0"]
["6GK5795-6MN01-0AA6","Mounting kit for ANT795-6MN Mounting aid for installation of ANT795-6MN below roof, IP20 (-40-+70 Β°C), Scope of delivery: 1 mounting aid 1 elbow adapter N-Connect male/female 2 mounting screws Compact instructions as hard copy German/English",86.399999999999991,"ST",1,"SIMATIC",1,"6GK57956MN010AA6"]
["6GK5992-4AM00-8AA0","SCALANCE X accessory; Media module MM992-4LD; 4x 1000 Mbit/s SC-ports, optical; single-mode optical up to max. 10 km",1460,"ST",1,"SIMATIC",1,"6GK59924AM008AA0"]
["6GT2398-1DC10","SIMATIC RF300/RF200 antenna ANT 12, stainless steel, IP65, -25 to +70 Β°C, thread M12x1, length 40 mm; with trailing antenna wire, both ends pluggable PUR, UL 758, length 3 m",363,"ST",1,"SIMATIC",1,"6GT23981DC10"]
["6GT2698-5AA10","MOBY D antenna ANT D5 to connection to SLG D10/SLG D10S and SLG D11/SLG D11S Basic units, incl. spacer; 380x 380x 110 mm (LxWxH) antenna wire 3.3 m enclosed",1073,"ST",1,"SIMATIC",1,"6GT26985AA10"]
["6GT2801-2BA10-0AX2","SIMATIC RF300; Reader RF340R (GEN2); RS422 interface (3964R); IP67, -25 to +70 Β°C, 75x 75x 41 mm with integrated antenna Special version ATEX (Zone 3G/3D) and IECEx (Gc/Dc) for Zone 2/22",892,"ST",1,"SIMATIC",1,"6GT28012BA100AX2"]
["6GT2821-4AC32","SIMATIC RF200 reader RF240R IO-Link IO-Link interface IP67, -25 to +70 Β°C; 50x 50x 30 mm; with integrated antenna 8 Byte IO; 38.4 Kbps",574,"ST",1,"SIMATIC",1,"6GT28214AC32"]
["6XV1801-5DH30","Power connecting cable M12-180/M12-180 for Power supply of the ET 200, pre-assembled cable with M12 connector and M12 socket, A-coded, 4-pole, 3.0 m",45.2,"ST",1,"SIMATIC",1,"6XV18015DH30"]
["6XV1830-0EN50","PROFIBUS FC Standard, bus cable 2-wire, shielded special configuration for Quick assembly 50 m",74,"ST",1,"SIMATIC",1,"6XV18300EN50"]
["6XV1860-3PH50","PROFIBUS ECOFAST Hybrid Cable GP, 2x Cu 0.64 mm, 4x Cu 1.5 mm2, Cable pre-assembled with ECOFAST connector and socket, trailable, Length 5 m",89.5,"ST",1,"SIMATIC",1,"6XV18603PH50"]
["6XV1871-5TH20","IE connecting cable M12-180/IE FC RJ45 Plug-145; IE FC Trailing cable GP pre-assembled with M12 connector (D-coded) and IE FC RJ45 plug; Length 2.0 m",44.7,"ST",1,"SIMATIC",1,"6XV18715TH20"]
["6XV1873-6AH30","FO Standard Cable GP (50/125), pre-assembled with 2x2 SC connectors, Length 3.0 m",70.399999999999991,"ST",1,"SIMATIC",1,"6XV18736AH30"]
["6XV1878-5SH30","IE TP Cord M12-90/RJ45-180, pre-assembled IE Flexible Cable, with 1x M12 connector (X-coded); 90 degrees cable outlet; 1x RJ45 connector; 180 degrees cable outlet; length 3.0 m",77.199999999999989,"ST",1,"SIMATIC",1,"6XV18785SH30"]
["RUM:ANTN0058-KIT","RUGGEDCOM ANTN0058-KIT GPS antenna (3.3 V) for use with WIN7200",337,"ST",1,"SIMATIC",1,"RUM:ANTN0058KIT"]
["RUM:WIN5225-5","RUGGEDCOM WIN5225-5 High Gain Outdoor Subscriber unit, integrated directional dual slant antenna includes commercial grade power supply, 2496 MHz to 2690 MHz",1439,"ST",1,"SIMATIC",1,"RUM:WIN52255"]
["6EP1436-3BA00-8AA0","SITOP modular plus 20 A Stabilized power supply input: 3 AC 400-500 V output: 24 V DC/20 A Option for with protective varnish",308,"ST",1,"SIMATIC",1,"6EP14363BA008AA0"]
["6EP3444-7SB00-3AX0","SITOP PSU6200 48 V/5 A Stabilized power supply Input: 400 - 500 V AC Output: 48 V DC/5 A With diagnostic interface",209,"ST",1,"SIMATIC",1,"6EP34447SB003AX0"]
["6ES7922-5BF00-0AB0","Front connector for SIMATIC S7-1500 40 pole (6ES7592-1AM00-0XB0) with 20 single cores 0.5 mm2 (1-20) Core type H05V-K Screw version L = 5.0 m",103,"ST",1,"SIMATIC",1,"6ES79225BF000AB0"]
["6ES7924-2CC20-0AC0","Connection module TPA 3-tier for analog Modules of the SIMATIC S7-1500 Type: Push-in terminal without LED, VPE=1 unit 50 pole IDC connector for cable",86.1,"ST",1,"SIMATIC",1,"6ES79242CC200AC0"]
["6ES7928-3CA20-4AA0","Relay for TPRO 230 V AC VPE = 4 units",56.7,"PAK",1,"SIMATIC",1,"6ES79283CA204AA0"]
["6ES7928-3DA20-4AA0","Relay for TPRO 60 VDC VPE = 4 units",60.9,"PAK",1,"SIMATIC",1,"6ES79283DA204AA0"]
["6ES7928-3EA20-4AA0","Relay for TPRI 110 V AC VPE = 4 units",56.7,"PAK",1,"SIMATIC",1,"6ES79283EA204AA0"]
["6ES7928-5AA20-4AA0","Enclosure cover for Connection module TP1  8-bit VPE = 4 units",12.9,"PAK",1,"SIMATIC",1,"6ES79285AA204AA0"]
["6ES7928-5BA20-4AA0","Enclosure cover for Connection modules TP2 / TP3 / TPA 8-bit VPE = 4 units",16.100000000000001,"PAK",1,"SIMATIC",1,"6ES79285BA204AA0"]
["6ES7928-5CA20-4AA0","Enclosure cover for Connection modules TP3 32-bit VPE = 4 units",23.6,"PAK",1,"SIMATIC",1,"6ES79285CA204AA0"]
["6ES7928-5DA20-4AA0","Enclosure cover for Connection modules TP1 32-bit / TP3 switch / TPRO 8-bit Packaging Unit = 4 PCs",17.200000000000003,"PAK",1,"SIMATIC",1,"6ES79285DA204AA0"]
["6ES7928-5EA20-4AA0","Enclosure cover for Connection modules TPA 32-bit / TP3 Fuse / TPRI / TPOO 8-bit Packaging Unit = 4 PCs",22.5,"PAK",1,"SIMATIC",1,"6ES79285EA204AA0"]
["6ES7928-6AA20-0AA0","Fuses 0.6 A VPE = 10 units",8.6999999999999993,"PAK",1,"SIMATIC",1,"6ES79286AA200AA0"]
["6XX3004","Screw terminal",35.300000000000004,"ST",1,"SIMATIC",1,"6XX3004"]
["6XX3070","crimp contacts for front connector K/490 (1 pack = 250 units)",48.6,"PAK",1,"SIMATIC",1,"6XX3070"]
["6XX3071","Crimping tool for crimping of crimp contacts for front connector K",711,"ST",1,"SIMATIC",1,"6XX3071"]
["7MF1566-3AB01-1AA1"," SITRANS P210 Transmitters for pressure and absolute pressure for low-pressure applications Non-linearity: 0,25 percent (typically) wetted parts material: stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 160 mbar, Overload- pressure 400 mbar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V with Explosion protection: EEx ia IIC T4 Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",480,"ΤΕΜ",1,"PI1",1,"7MF15663AB011AA1"]
["7MF1566-3AB00-1AA1"," SITRANS P210 Transmitters for pressure and absolute pressure for low-pressure applications Non-linearity: 0,25 percent (typically) wetted parts material: stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 160 mbar, Overload- pressure 400 mbar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V without explosion protection Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",439,"ΤΕΜ",1,"PI1",1,"7MF15663AB001AA1"]
["7MF1566-3AB01-1AA1"," SITRANS P210 Transmitters for pressure and absolute pressure for low-pressure applications Non-linearity: 0,25 percent (typically) wetted parts material: stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 160 mbar, Overload- pressure 400 mbar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V with Explosion protection: EEx ia IIC T4 Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",480,"ΤΕΜ",1,"PI1",1,"7MF15663AB011AA1"]
["7MF1566-3AC00-1AA1"," SITRANS P210 Transmitters for pressure and absolute pressure for low-pressure applications Non-linearity: 0,25 percent (typically) wetted parts material: stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 250 mbar, Overload- pressure 1000 mbar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V without explosion protection Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",439,"ΤΕΜ",1,"PI1",1,"7MF15663AC001AA1"]
["7MF1566-3AC01-1AA1"," SITRANS P210 Transmitters for pressure and absolute pressure for low-pressure applications Non-linearity: 0,25 percent (typically) wetted parts material: stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 250 mbar, Overload- pressure 1000 mbar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V with Explosion protection: EEx ia IIC T4 Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",480,"ΤΕΜ",1,"PI1",1,"7MF15663AC011AA1"]
["7MF1566-3AD00-1AA1"," SITRANS P210 Transmitters for pressure and absolute pressure for low-pressure applications Non-linearity: 0,25 percent (typically) wetted parts material: stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 400 mbar, Overload- pressure 1000 mbar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V without explosion protection Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",439,"ΤΕΜ",1,"PI1",1,"7MF15663AD001AA1"]
["7MF1566-3AD01-1AA1"," SITRANS P210 Transmitters for pressure and absolute pressure for low-pressure applications Non-linearity: 0,25 percent (typically) wetted parts material: stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 400 mbar, Overload- pressure 1000 mbar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V with Explosion protection: EEx ia IIC T4 Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",480,"ΤΕΜ",1,"PI1",1,"7MF15663AD011AA1"]
["7MF1566-3AG00-1AA1"," SITRANS P210 Transmitters for pressure and absolute pressure for low-pressure applications Non-linearity: 0,25 percent (typically) wetted parts material: stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range: Special version, in plain text. Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V Explosion protection: EEx ia Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: 1/4\"-18 NPT male (standard for pressure ranges psi) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",439,"ΤΕΜ",1,"PI1",1,"7MF15663AG001AA1"]
["7MF1566-3AG01-1AA1"," SITRANS P210 Transmitters for pressure and absolute pressure for low-pressure applications Non-linearity: 0,25 percent (typically) wetted parts material: stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 600 mbar, Overload- pressure 2000 mbar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V with Explosion protection: EEx ia IIC T4 Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",480,"ΤΕΜ",1,"PI1",1,"7MF15663AG011AA1"]
["7MF1565-3BA00-1AA1"," SITRANS P200 Transmitters for pressure and absolute pressure for general applications Non-linearity: 0,25 percent (typically) wetted parts material:ceramics, stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 1 bar, Overload- pressure 2,5 bar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V without explosion protection Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",181,"ΤΕΜ",1,"PI1",1,"7MF15653BA001AA1"]
["7MF1565-3BA01-1AA1"," SITRANS P200 Transmitters for pressure and absolute pressure for general applications Non-linearity: 0,25 percent (typically) wetted parts material:ceramics, stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 1 bar, Overload- pressure 2,5 bar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V with Explosion protection: EEx ia IIC T4 Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",218,"ΤΕΜ",1,"PI1",1,"7MF15653BA011AA1"]
["7MF1565-3BB00-1AA1"," SITRANS P200 Transmitters for pressure and absolute pressure for general applications Non-linearity: 0,25 percent (typically) wetted parts material:ceramics, stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 1.6 bar, Overload- pressure 4 bar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V without explosion protection Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",181,"ΤΕΜ",1,"PI1",1,"7MF15653BB001AA1"]
["7MF1565-3BB01-1AA1"," SITRANS P200 Transmitters for pressure and absolute pressure for general applications Non-linearity: 0,25 percent (typically) wetted parts material:ceramics, stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 1.6 bar, Overload- pressure 4 bar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V with Explosion protection: EEx ia IIC T4 Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",218,"ΤΕΜ",1,"PI1",1,"7MF15653BB011AA1"]
["7MF1565-3BD00-1AA1"," SITRANS P200 Transmitters for pressure and absolute pressure for general applications Non-linearity: 0,25 percent (typically) wetted parts material:ceramics, stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 2,5 bar, Overload- pressure 6,25 bar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V without explosion protection Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",181,"ΤΕΜ",1,"PI1",1,"7MF15653BD001AA1"]
["7MF1565-3BD01-1AA1"," SITRANS P200 Transmitters for pressure and absolute pressure for general applications Non-linearity: 0,25 percent (typically) wetted parts material:ceramics, stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 2,5 bar, Overload- pressure 6,25 bar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V with Explosion protection: EEx ia IIC T4 Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",218,"ΤΕΜ",1,"PI1",1,"7MF15653BD011AA1"]
["7MF1565-3BE00-1AA1"," SITRANS P200 Transmitters for pressure and absolute pressure for general applications Non-linearity: 0,25 percent (typically) wetted parts material:ceramics, stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 4 bar, Overload- pressure 10 bar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V without explosion protection Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",181,"ΤΕΜ",1,"PI1",1,"7MF15653BE001AA1"]
["7MF1565-3BE01-1AA1"," SITRANS P200 Transmitters for pressure and absolute pressure for general applications Non-linearity: 0,25 percent (typically) wetted parts material:ceramics, stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 4 bar, Overload- pressure 10 bar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V with Explosion protection: EEx ia IIC T4 Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",218,"ΤΕΜ",1,"PI1",1,"7MF15653BE011AA1"]
["7MF1565-3BG00-1AA1"," SITRANS P200 Transmitters for pressure and absolute pressure for general applications Non-linearity: 0,25 percent (typically) wetted parts material:ceramics, stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 6 bar, Overload- pressure 15 bar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V without explosion protection Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",181,"ΤΕΜ",1,"PI1",1,"7MF15653BG001AA1"]
["7MF1565-3BG01-1AA1"," SITRANS P200 Transmitters for pressure and absolute pressure for general applications Non-linearity: 0,25 percent (typically) wetted parts material:ceramics, stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 6 bar, Overload- pressure 15 bar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V with Explosion protection: EEx ia IIC T4 Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",218,"ΤΕΜ",1,"PI1",1,"7MF15653BG011AA1"]
["7MF1565-3CA00-1AA1"," SITRANS P200 Transmitters for pressure and absolute pressure for general applications Non-linearity: 0,25 percent (typically) wetted parts material:ceramics, stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 10 bar, Overload- pressure 25 bar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V without explosion protection Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",181,"ΤΕΜ",1,"PI1",1,"7MF15653CA001AA1"]
["7MF1565-3CA01-1AA1"," SITRANS P200 Transmitters for pressure and absolute pressure for general applications Non-linearity: 0,25 percent (typically) wetted parts material:ceramics, stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 10 bar, Overload- pressure 25 bar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V with Explosion protection: EEx ia IIC T4 Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",218,"ΤΕΜ",1,"PI1",1,"7MF15653CA011AA1"]
["7MF1565-3CB00-1AA1"," SITRANS P200 Transmitters for pressure and absolute pressure for general applications Non-linearity: 0,25 percent (typically) wetted parts material:ceramics, stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 16 bar, Overload- pressure 40 bar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V without explosion protection Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",181,"ΤΕΜ",1,"PI1",1,"7MF15653CB001AA1"]
["7MF1565-3CB01-1AA1"," SITRANS P200 Transmitters for pressure and absolute pressure for general applications Non-linearity: 0,25 percent (typically) wetted parts material:ceramics, stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 16 bar, Overload- pressure 40 bar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V with Explosion protection: EEx ia IIC T4 Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",218,"ΤΕΜ",1,"PI1",1,"7MF15653CB011AA1"]
["7MF1565-3CD00-1AA1"," SITRANS P200 Transmitters for pressure and absolute pressure for general applications Non-linearity: 0,25 percent (typically) wetted parts material:ceramics, stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 25 bar, Overload- pressure 62,5 bar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V without explosion protection Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",181,"ΤΕΜ",1,"PI1",1,"7MF15653CD001AA1"]
["7MF1565-3CD01-1AA1"," SITRANS P200 Transmitters for pressure and absolute pressure for general applications Non-linearity: 0,25 percent (typically) wetted parts material:ceramics, stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 25 bar, Overload- pressure 62,5 bar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V with Explosion protection: EEx ia IIC T4 Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",218,"ΤΕΜ",1,"PI1",1,"7MF15653CD011AA1"]
["7MF1565-3CE00-1AA1"," SITRANS P200 Transmitters for pressure and absolute pressure for general applications Non-linearity: 0,25 percent (typically) wetted parts material:ceramics, stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 40 bar, Overload- pressure 100 bar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V without explosion protection Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",181,"ΤΕΜ",1,"PI1",1,"7MF15653CE001AA1"]
["7MF1565-3CE01-1AA1"," SITRANS P200 Transmitters for pressure and absolute pressure for general applications Non-linearity: 0,25 percent (typically) wetted parts material:ceramics, stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 40 bar, Overload- pressure 100 bar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V with Explosion protection: EEx ia IIC T4 Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",218,"ΤΕΜ",1,"PI1",1,"7MF15653CE011AA1"]
["7MF1565-3CG00-1AA1"," SITRANS P200 Transmitters for pressure and absolute pressure for general applications Non-linearity: 0,25 percent (typically) wetted parts material:ceramics, stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 60 bar, Overload- pressure 150 bar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V without explosion protection Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",181,"ΤΕΜ",1,"PI1",1,"7MF15653CG001AA1"]
["7MF1565-3CG01-1AA1"," SITRANS P200 Transmitters for pressure and absolute pressure for general applications Non-linearity: 0,25 percent (typically) wetted parts material:ceramics, stainless steel plus sealing material; non-wetted parts material: stainless steel Measuring range for gauge: 0 to 60 bar, Overload- pressure 150 bar Output signal: 4 to 20 mA two-wire connection, power supply DC 7 to 33 V with Explosion protection: EEx ia IIC T4 Electrical connection: plug to DIN EN 175301-803-A, threat for packed gland M16 (with connector) Process connection: G1/2\" male to EN 837-1 (1/2\" BSP male) (standard for metric pressure ranges mbar, bar) Sealing material between sensor and housing: Viton (FPM, Standard) Standard version",218,"ΤΕΜ",1,"PI1",1,"7MF15653CG011AA1"]
["M56340-A0059","PRESSURE IMPACT REDUCER STAINLESS STEEL",52,"ΤΕΜ",1,"PI1",1,"M56340A0059"]
["7MF1572-1CA20","Transmitters SITRANS LH100 for hydrostatic level measurement, submersible transmitter, two-wire connection, 4...20 mA housing material 316L (1.4404) measuring cell ceramics (96%) with fixed mounted LD-PE cable Measuring range: 0 - 3 mH2O Cable lenght: 10 m . . Sealing material between sensor and housing: EPDM (for drinking water) Without explosion proof ",559,"ΤΕΜ",1,"PI1",1,"7MF15721CA20"]
["7MF1572-1CA21","Transmitters SITRANS LH100 for hydrostatic level measurement, submersible transmitter, two-wire connection, 4...20 mA housing material 316L (1.4404) measuring cell ceramics (96%) with fixed mounted LD-PE cable Measuring range: 0 - 3 mH2O Cable lenght: 10 m . . Sealing material between sensor and housing: EPDM (for drinking water) with ATEX II1 G Ex ia IIC T4 Ga and IECEx Ex ia IIC T4 Ga ",615,"ΤΕΜ",1,"PI1",1,"7MF15721CA21"]
["7MF1572-1DA10","Transmitters SITRANS LH100 for hydrostatic level measurement, submersible transmitter, two-wire connection, 4...20 mA housing material 316L (1.4404) measuring cell ceramics (96%) with fixed mounted LD-PE cable Measuring range: 0 - 4 mH2O Cable lenght: 10 m . . Sealing material between sensor and housing: FPM (standard) Without explosion proof ",559,"ΤΕΜ",1,"PI1",1,"7MF15721DA10"]
["7MF1572-1DA11","Transmitters SITRANS LH100 for hydrostatic level measurement, submersible transmitter, two-wire connection, 4...20 mA housing material 316L (1.4404) measuring cell ceramics (96%) with fixed mounted LD-PE cable Measuring range: 0 - 4 mH2O Cable lenght: 10 m . . Sealing material between sensor and housing: FPM (standard) with ATEX II1 G Ex ia IIC T4 Ga and IECEx Ex ia IIC T4 Ga ",615,"ΤΕΜ",1,"PI1",1,"7MF1572-1DA11"]
["7MF1572-1DA20","Transmitters SITRANS LH100 for hydrostatic level measurement, submersible transmitter, two-wire connection, 4...20 mA housing material 316L (1.4404) measuring cell ceramics (96%) with fixed mounted LD-PE cable Measuring range: 0 - 4 mH2O Cable lenght: 10 m . . Sealing material between sensor and housing: EPDM (for drinking water) Without explosion proof ",559,"ΤΕΜ",1,"PI1",1,"7MF15721DA20"]
["7MF1572-1DA21","Transmitters SITRANS LH100 for hydrostatic level measurement, submersible transmitter, two-wire connection, 4...20 mA housing material 316L (1.4404) measuring cell ceramics (96%) with fixed mounted LD-PE cable Measuring range: 0 - 4 mH2O Cable lenght: 10 m . . Sealing material between sensor and housing: EPDM (for drinking water) with ATEX II1 G Ex ia IIC T4 Ga and IECEx Ex ia IIC T4 Ga ",615,"ΤΕΜ",1,"PI1",1,"7MF1572-1DA21"]
["7MF1572-1EA10","Transmitters SITRANS LH100 for hydrostatic level measurement, submersible transmitter, two-wire connection, 4...20 mA housing material 316L (1.4404) measuring cell ceramics (96%) with fixed mounted LD-PE cable Measuring range: 0 - 5 mH2O Cable lenght: 10 m . . Sealing material between sensor and housing: FPM (standard) Without explosion proof ",559,"ΤΕΜ",1,"PI1",1,"7MF15721EA10"]
["7MF1572-1EA11","Transmitters SITRANS LH100 for hydrostatic level measurement, submersible transmitter, two-wire connection, 4...20 mA housing material 316L (1.4404) measuring cell ceramics (96%) with fixed mounted LD-PE cable Measuring range: 0 - 5 mH2O Cable lenght: 10 m . . Sealing material between sensor and housing: FPM (standard) with ATEX II1 G Ex ia IIC T4 Ga and IECEx Ex ia IIC T4 Ga ",615,"ΤΕΜ",1,"PI1",1,"7MF1572-1EA11"]
["7MF1572-1EA20","Transmitters SITRANS LH100 for hydrostatic level measurement, submersible transmitter, two-wire connection, 4...20 mA housing material 316L (1.4404) measuring cell ceramics (96%) with fixed mounted LD-PE cable Measuring range: 0 - 5 mH2O Cable lenght: 10 m . . Sealing material between sensor and housing: EPDM (for drinking water) Without explosion proof ",559,"ΤΕΜ",1,"PI1",1,"7MF15721EA20"]
["7MF1572-1EA21","Transmitters SITRANS LH100 for hydrostatic level measurement, submersible transmitter, two-wire connection, 4...20 mA housing material 316L (1.4404) measuring cell ceramics (96%) with fixed mounted LD-PE cable Measuring range: 0 - 5 mH2O Cable lenght: 10 m . . Sealing material between sensor and housing: FPM (standard) with ATEX II1 G Ex ia IIC T4 Ga and IECEx Ex ia IIC T4 Ga ",615,"ΤΕΜ",1,"PI1",1,"7MF15721EA21"]
["7MF1572-1FA10","Transmitters SITRANS LH100 for hydrostatic level measurement, submersible transmitter, two-wire connection, 4...20 mA housing material 316L (1.4404) measuring cell ceramics (96%) with fixed mounted LD-PE cable Measuring range: 0 - 6 mH2O Cable lenght: 10 m . . Sealing material between sensor and housing: FPM (standard) Without explosion proof ",559,"ΤΕΜ",1,"PI1",1,"7MF15721FA10"]
["7MF1572-1FA11","Transmitters SITRANS LH100 for hydrostatic level measurement, submersible transmitter, two-wire connection, 4...20 mA housing material 316L (1.4404) measuring cell ceramics (96%) with fixed mounted LD-PE cable Measuring range: 0 - 6 mH2O Cable lenght: 10 m . . Sealing material between sensor and housing: FPM (standard) with ATEX II1 G Ex ia IIC T4 Ga and IECEx Ex ia IIC T4 Ga ",615,"ΤΕΜ",1,"PI1",1,"7MF15721FA11"]
["7MF1572-1FA20","Transmitters SITRANS LH100 for hydrostatic level measurement, submersible transmitter, two-wire connection, 4...20 mA housing material 316L (1.4404) measuring cell ceramics (96%) with fixed mounted LD-PE cable Measuring range: 0 - 6 mH2O Cable lenght: 10 m . . Sealing material between sensor and housing: EPDM (for drinking water) Without explosion proof ",559,"ΤΕΜ",1,"PI1",1,"7MF15721FA20"]
["7MF1572-1FA21","Transmitters SITRANS LH100 for hydrostatic level measurement, submersible transmitter, two-wire connection, 4...20 mA housing material 316L (1.4404) measuring cell ceramics (96%) with fixed mounted LD-PE cable Measuring range: 0 - 6 mH2O Cable lenght: 10 m . . Sealing material between sensor and housing: EPDM (for drinking water)  with ATEX II1 G Ex ia IIC T4 Ga and IECEx Ex ia IIC T4 Ga ",615,"ΤΕΜ",1,"PI1",1,"7MF15721FA21"]
["7MF1572-1HA10","Transmitters SITRANS LH100 for hydrostatic level measurement, submersible transmitter, two-wire connection, 4...20 mA housing material 316L (1.4404) measuring cell ceramics (96%) with fixed mounted LD-PE cable Measuring range: 0 - 10 mH2O Cable lenght: 25 m . . Sealing material between sensor and housing: FPM (standard) Without explosion proof ",643,"ΤΕΜ",1,"PI1",1,"7MF15721HA10"]
["7MF1572-1HA11","Transmitters SITRANS LH100 for hydrostatic level measurement, submersible transmitter, two-wire connection, 4...20 mA housing material 316L (1.4404) measuring cell ceramics (96%) with fixed mounted LD-PE cable Measuring range: 0 - 10 mH2O Cable lenght: 25 m . . Sealing material between sensor and housing: FPM (standard) with ATEX II1 G Ex ia IIC T4 Ga and IECEx Ex ia IIC T4 Ga ",699,"ΤΕΜ",1,"PI1",1,"7MF15721HA11"]
["7MF1572-1HA20","Transmitters SITRANS LH100 for hydrostatic level measurement, submersible transmitter, two-wire connection, 4...20 mA housing material 316L (1.4404) measuring cell ceramics (96%) with fixed mounted LD-PE cable Measuring range: 0 - 10 mH2O Cable lenght: 25 m . . Sealing material between sensor and housing: EPDM (for drinking water) Without explosion proof ",643,"ΤΕΜ",1,"PI1",1,"7MF15721HA20"]
["7MF1572-1HA21","Transmitters SITRANS LH100 for hydrostatic level measurement, submersible transmitter, two-wire connection, 4...20 mA housing material 316L (1.4404) measuring cell ceramics (96%) with fixed mounted LD-PE cable Measuring range: 0 - 10 mH2O Cable lenght: 20 m . . Sealing material between sensor and housing: EPDM (for drinking water) with ATEX II1 G Ex ia IIC T4 Ga and IECEx Ex ia IIC T4 Ga ",699,"ΤΕΜ",1,"PI1",1,"7MF15721HA21"]
["7MF1572-1KA10","Transmitters SITRANS LH100 for hydrostatic level measurement, submersible transmitter, two-wire connection, 4...20 mA housing material 316L (1.4404) measuring cell ceramics (96%) with fixed mounted LD-PE cable Measuring range: 0 - 20 mH2O Cable lenght: 30 m . . Sealing material between sensor and housing: FPM (standard) with ATEX II1 G Ex ia IIC T4 Ga and IECEx Ex ia IIC T4 Ga ",731,"ΤΕΜ",1,"PI1",1,"7MF15721KA10"]
["7MF1572-1KA11","Transmitters SITRANS LH100 for hydrostatic level measurement, submersible transmitter, two-wire connection, 4...20 mA housing material 316L (1.4404) measuring cell ceramics (96%) with fixed mounted LD-PE cable Measuring range: 0 - 20 mH2O Cable lenght: 30 m . . Sealing material between sensor and housing: EPDM (for drinking water) Without explosion proof ",787,"ΤΕΜ",1,"PI1",1,"7MF15721KA11"]
["7MF1572-1KA20","Transmitters SITRANS LH100 for hydrostatic level measurement, submersible transmitter, two-wire connection, 4...20 mA housing material 316L (1.4404) measuring cell ceramics (96%) with fixed mounted LD-PE cable Measuring range: 0 - 20 mH2O Cable lenght: 30 m . . Sealing material between sensor and housing: EPDM (for drinking water) Without explosion proof ",731,"ΤΕΜ",1,"PI1",1,"7MF15721KA20"]
["7MF1572-1KA21","Transmitters SITRANS LH100 for hydrostatic level measurement, submersible transmitter, two-wire connection, 4...20 mA housing material 316L (1.4404) measuring cell ceramics (96%) with fixed mounted LD-PE cable Measuring range: 0 - 20 mH2O Cable lenght: 30 m . . Sealing material between sensor and housing: EPDM (for drinking water) with ATEX II1 G Ex ia IIC T4 Ga and IECEx Ex ia IIC T4 Ga ",787,"ΤΕΜ",1,"PI1",1,"7MF15721KA21"]
["7MF1572-8AA","CABLE BOX FOR CONNECTION OF 7MF1572* MEASUREMENT TRANSDUCER WITH VENTILATION Degree of protection IP54 Material: PLASTIC",70,"ΤΕΜ",1,"PI1",1,"7MF15728AA"]
["7MF1572-8AB","ANCHOR CLAMP FOR ATTACHMENT OF 7MF1572* MEASUREMENT TRANSDUCER Material: STEEL COATED",16,"ΤΕΜ",1,"PI1",1,"7MF15728AB"]
["7MF8010-1AD31-1BB1","SITRANS P Transmitter Compact for pressure and absolut pressure for food, pharmaceu- ticals and biotechnology, with diaphragm flush at front. 2-wire system, process tempera- ture up to 140 deg. Cel., accuracy 0.2 % of f.s.v. output signal: 4...20 mA, Process connection: quick-release connection: connection o.cc.according DIN 11851 with slotted union nut: DN 25 Filling liquid: liquid FDA approved Output signal : 4-20 mA Housing(stainless steel1.4404)/ electrical connection: housing with angeld plug according DIN 43650, IP65 Measuring range: 0...160 mbar overload pressure: 1 bar Without explosion protection ",463,"ΤΕΜ",1,"PI1",1,"7MF80101AD311BB1"]
["7MF8010-1AD31-1BC1","SITRANS P Transmitter Compact for pressure and absolut pressure for food, pharmaceu- ticals and biotechnology, with diaphragm flush at front. 2-wire system, process tempera- ture up to 140 deg. Cel., accuracy 0.2 % of f.s.v. output signal: 4...20 mA, Process connection: quick-release connection: connection o.cc.according DIN 11851 with slotted union nut: DN 25 Filling liquid: liquid FDA approved Output signal : 4-20 mA Housing(stainless steel1.4404)/ electrical connection: housing with angeld plug according DIN 43650, IP65 Measuring range: 0...250 mbar overload pressure: 1 bar Without explosion protection ",463,"ΤΕΜ",1,"PI1",1,"7MF80101AD311BC1"]
["7MF8010-1AD31-1BD1","SITRANS P Transmitter Compact for pressure and absolut pressure for food, pharmaceu- ticals and biotechnology, with diaphragm flush at front. 2-wire system, process tempera- ture up to 140 deg. Cel., accuracy 0.2 % of f.s.v. output signal: 4...20 mA, Process connection: quick-release connection: connection o.cc.according DIN 11851 with slotted union nut: DN 25 Filling liquid: liquid FDA approved Output signal : 4-20 mA Housing(stainless steel1.4404)/ electrical connection: housing with angeld plug according DIN 43650, IP65 Measuring range: 0...400 mbar overload pressure: 3 bar Without explosion protection ",463,"ΤΕΜ",1,"PI1",1,"7MF80101AD311BD1"]
["7MF8010-1AD31-1BE1","SITRANS P Transmitter Compact for pressure and absolut pressure for food, pharmaceu- ticals and biotechnology, with diaphragm flush at front. 2-wire system, process tempera- ture up to 140 deg. Cel., accuracy 0.2 % of f.s.v. output signal: 4...20 mA, Process connection: quick-release connection: connection o.cc.according DIN 11851 with slotted union nut: DN 25 Filling liquid: liquid FDA approved Output signal : 4-20 mA Housing(stainless steel1.4404)/ electrical connection: housing with angeld plug according DIN 43650, IP65 Measuring range: 0...600 mbar overload pressure: 3 bar Without explosion protection ",463,"ΤΕΜ",1,"PI1",1,"7MF80101AD311BE1"]
["7MF8010-1AD31-1CA1","SITRANS P Transmitter Compact for pressure and absolut pressure for food, pharmaceu- ticals and biotechnology, with diaphragm flush at front. 2-wire system, process tempera- ture up to 140 deg. Cel., accuracy 0.2 % of f.s.v. output signal: 4...20 mA, Process connection: quick-release connection: connection o.cc.according DIN 11851 with slotted union nut: DN 25 Filling liquid: liquid FDA approved Output signal : 4-20 mA Housing(stainless steel1.4404)/ electrical connection: housing with angeld plug according DIN 43650, IP65 Measuring range: 0...1 bar overload pressure: 3 bar Without explosion protection ",463,"ΤΕΜ",1,"PI1",1,"7MF80101AD311CA1"]
["7MF8010-1AD31-1CB1","SITRANS P Transmitter Compact for pressure and absolut pressure for food, pharmaceu- ticals and biotechnology, with diaphragm flush at front. 2-wire system, process tempera- ture up to 140 deg. Cel., accuracy 0.2 % of f.s.v. output signal: 4...20 mA, Process connection: quick-release connection: connection o.cc.according DIN 11851 with slotted union nut: DN 25 Filling liquid: liquid FDA approved Output signal : 4-20 mA Housing(stainless steel1.4404)/ electrical connection: housing with angeld plug according DIN 43650, IP65 Measuring range: 0...1,6 bar overload pressure: 10 bar Without explosion protection ",463,"ΤΕΜ",1,"PI1",1,"7MF80101AD311CB1"]
["7MF8010-1AD31-1CC1","SITRANS P Transmitter Compact for pressure and absolut pressure for food, pharmaceu- ticals and biotechnology, with diaphragm flush at front. 2-wire system, process tempera- ture up to 140 deg. Cel., accuracy 0.2 % of f.s.v. output signal: 4...20 mA, Process connection: quick-release connection: connection o.cc.according DIN 11851 with slotted union nut: DN 25 Filling liquid: liquid FDA approved Output signal : 4-20 mA Housing(stainless steel1.4404)/ electrical connection: housing with angeld plug according DIN 43650, IP65 Measuring range: 0...2,5 bar overload pressure: 10 bar Without explosion protection ",463,"ΤΕΜ",1,"PI1",1,"7MF80101AD311CC1"]
["7MF8010-1AD31-1CD1","SITRANS P Transmitter Compact for pressure and absolut pressure for food, pharmaceu- ticals and biotechnology, with diaphragm flush at front. 2-wire system, process tempera- ture up to 140 deg. Cel., accuracy 0.2 % of f.s.v. output signal: 4...20 mA, Process connection: quick-release connection: connection o.cc.according DIN 11851 with slotted union nut: DN 25 Filling liquid: liquid FDA approved Output signal : 4-20 mA Housing(stainless steel1.4404)/ electrical connection: housing with angeld plug according DIN 43650, IP65 Measuring range: 0...4 bar overload pressure: 20 bar Without explosion protection ",463,"ΤΕΜ",1,"PI1",1,"7MF80101AD311CD1"]
["7MF8010-1AD31-1CE1","SITRANS P Transmitter Compact for pressure and absolut pressure for food, pharmaceu- ticals and biotechnology, with diaphragm flush at front. 2-wire system, process tempera- ture up to 140 deg. Cel., accuracy 0.2 % of f.s.v. output signal: 4...20 mA, Process connection: quick-release connection: connection o.cc.according DIN 11851 with slotted union nut: DN 25 Filling liquid: liquid FDA approved Output signal : 4-20 mA Housing(stainless steel1.4404)/ electrical connection: housing with angeld plug according DIN 43650, IP65 Measuring range: 0...6 bar overload pressure: 60 bar Without explosion protection ",463,"ΤΕΜ",1,"PI1",1,"7MF80101AD311CE1"]
["7MF8010-1AD31-1DA1","SITRANS P Transmitter Compact for pressure and absolut pressure for food, pharmaceu- ticals and biotechnology, with diaphragm flush at front. 2-wire system, process tempera- ture up to 140 deg. Cel., accuracy 0.2 % of f.s.v. output signal: 4...20 mA, Process connection: quick-release connection: connection o.cc.according DIN 11851 with slotted union nut: DN 25 Filling liquid: liquid FDA approved Output signal : 4-20 mA Housing(stainless steel1.4404)/ electrical connection: housing with angeld plug according DIN 43650, IP65 Measuring range: 0...10 bar overload pressure: 60 bar Without explosion protection ",463,"ΤΕΜ",1,"PI1",1,"7MF80101AD311DA1"]
["7MF8010-1AD31-1DB1","SITRANS P Transmitter Compact for pressure and absolut pressure for food, pharmaceu- ticals and biotechnology, with diaphragm flush at front. 2-wire system, process tempera- ture up to 140 deg. Cel., accuracy 0.2 % of f.s.v. output signal: 4...20 mA, Process connection: quick-release connection: connection o.cc.according DIN 11851 with slotted union nut: DN 25 Filling liquid: liquid FDA approved Output signal : 4-20 mA Housing(stainless steel1.4404)/ electrical connection: housing with angeld plug according DIN 43650, IP65 Measuring range: 0...16 bar overload pressure: 60 bar Without explosion protection ",463,"ΤΕΜ",1,"PI1",1,"7MF80101AD311DB1"]
["7MF8010-1AD31-1DC1","SITRANS P Transmitter Compact for pressure and absolut pressure for food, pharmaceu- ticals and biotechnology, with diaphragm flush at front. 2-wire system, process tempera- ture up to 140 deg. Cel., accuracy 0.2 % of f.s.v. output signal: 4...20 mA, Process connection: quick-release connection: connection o.cc.according DIN 11851 with slotted union nut: DN 25 Filling liquid: liquid FDA approved Output signal : 4-20 mA Housing(stainless steel1.4404)/ electrical connection: housing with angeld plug according DIN 43650, IP65 Measuring range: 0...25 bar overload pressure: 60 bar Without explosion protection ",463,"ΤΕΜ",1,"PI1",1,"7MF80101AD311DC1"]
["7MF8010-1AD31-1DD1","SITRANS P Transmitter Compact for pressure and absolut pressure for food, pharmaceu- ticals and biotechnology, with diaphragm flush at front. 2-wire system, process tempera- ture up to 140 deg. Cel., accuracy 0.2 % of f.s.v. output signal: 4...20 mA, Process connection: quick-release connection: connection o.cc.according DIN 11851 with slotted union nut: DN 25 Filling liquid: liquid FDA approved Output signal : 4-20 mA Housing(stainless steel1.4404)/ electrical connection: housing with angeld plug according DIN 43650, IP65 Measuring range: 0...40 bar overload pressure: 100 bar Without explosion protection ",463,"ΤΕΜ",1,"PI1",1,"7MF80101AD311DD1"]
["7MF8010-1AD31-1EB1"," SITRANS P Transmitter Compact for pressure and absolut pressure for food, pharmaceu- ticals and biotechnology, with diaphragm flush at front. 2-wire system, process tempera- ture up to 140 deg. Cel., accuracy 0.2 % of f.s.v. output signal: 4...20 mA, Process connection: quick-release connection: connection o.cc.according DIN 11851 with slotted union nut: DN 25 Filling liquid: liquid FDA approved Output signal : 4-20 mA Housing(stainless steel1.4404)/ electrical connection: housing with angeld plug according DIN 43650, IP65 Measuring range: -160...0 mbar overload pressure: 1 bar Without explosion protection",463,"ΤΕΜ",1,"PI1",1,"7MF80101AD311EB1"]
["7MF8010-1AD31-1EC1","SITRANS P Transmitter Compact for pressure and absolut pressure for food, pharmaceu- ticals and biotechnology, with diaphragm flush at front. 2-wire system, process tempera- ture up to 140 deg. Cel., accuracy 0.2 % of f.s.v. output signal: 4...20 mA, Process connection: quick-release connection: connection o.cc.according DIN 11851 with slotted union nut: DN 25 Filling liquid: liquid FDA approved Output signal : 4-20 mA Housing(stainless steel1.4404)/ electrical connection: housing with angeld plug according DIN 43650, IP65 Measuring range: -250...0 mbar overload pressure: 1 bar Without explosion protection ",463,"ΤΕΜ",1,"PI1",1,"7MF80101AD311EC1"]
["7MF8010-1AD31-1ED1","SITRANS P Transmitter Compact for pressure and absolut pressure for food, pharmaceu- ticals and biotechnology, with diaphragm flush at front. 2-wire system, process tempera- ture up to 140 deg. Cel., accuracy 0.2 % of f.s.v. output signal: 4...20 mA, Process connection: quick-release connection: connection o.cc.according DIN 11851 with slotted union nut: DN 25 Filling liquid: liquid FDA approved Output signal : 4-20 mA Housing(stainless steel1.4404)/ electrical connection: housing with angeld plug according DIN 43650, IP65 Measuring range: -400...0 mbar overload pressure: 3 bar Without explosion protection ",463,"ΤΕΜ",1,"PI1",1,"7MF80101AD311ED1"]
["7MF8010-1AD31-1EE1","SITRANS P Transmitter Compact for pressure and absolut pressure for food, pharmaceu- ticals and biotechnology, with diaphragm flush at front. 2-wire system, process tempera- ture up to 140 deg. Cel., accuracy 0.2 % of f.s.v. output signal: 4...20 mA, Process connection: quick-release connection: connection o.cc.according DIN 11851 with slotted union nut: DN 25 Filling liquid: liquid FDA approved Output signal : 4-20 mA Housing(stainless steel1.4404)/ electrical connection: housing with angeld plug according DIN 43650, IP65 Measuring range: -600...0 mbar overload pressure: 3 bar Without explosion protection ",463,"ΤΕΜ",1,"PI1",1,"7MF80101AD311EE1"]
["7MF8010-1AD31-1FA1","SITRANS P Transmitter Compact for pressure and absolut pressure for food, pharmaceu- ticals and biotechnology, with diaphragm flush at front. 2-wire system, process tempera- ture up to 140 deg. Cel., accuracy 0.2 % of f.s.v. output signal: 4...20 mA, Process connection: quick-release connection: connection o.cc.according DIN 11851 with slotted union nut: DN 25 Filling liquid: liquid FDA approved Output signal : 4-20 mA Housing(stainless steel1.4404)/ electrical connection: housing with angeld plug according DIN 43650, IP65 Measuring range: -1...0 bar overload pressure: 3 bar Without explosion protection ",463,"ΤΕΜ",1,"PI1",1,"7MF80101AD311FA1"]
["7MF8010-1AD31-1FB1","SITRANS P Transmitter Compact for pressure and absolut pressure for food, pharmaceu- ticals and biotechnology, with diaphragm flush at front. 2-wire system, process tempera- ture up to 140 deg. Cel., accuracy 0.2 % of f.s.v. output signal: 4...20 mA, Process connection: quick-release connection: connection o.cc.according DIN 11851 with slotted union nut: DN 25 Filling liquid: liquid FDA approved Output signal : 4-20 mA Housing(stainless steel1.4404)/ electrical connection: housing with angeld plug according DIN 43650, IP65 Measuring range: -1...0,6 bar overload pressure: 10 bar Without explosion protection ",463,"ΤΕΜ",1,"PI1",1,"7MF80101AD311FB1"]
["7MF8010-1AD31-1FC1","SITRANS P Transmitter Compact for pressure and absolut pressure for food, pharmaceu- ticals and biotechnology, with diaphragm flush at front. 2-wire system, process tempera- ture up to 140 deg. Cel., accuracy 0.2 % of f.s.v. output signal: 4...20 mA, Process connection: quick-release connection: connection o.cc.according DIN 11851 with slotted union nut: DN 25 Filling liquid: liquid FDA approved Output signal : 4-20 mA Housing(stainless steel1.4404)/ electrical connection: housing with angeld plug according DIN 43650, IP65 Measuring range: -1...1,5 bar overload pressure: 10 bar Without explosion protection ",463,"ΤΕΜ",1,"PI1",1,"7MF80101AD311FC1"]
["7MF8010-1AD31-1FD1","SITRANS P Transmitter Compact for pressure and absolut pressure for food, pharmaceu- ticals and biotechnology, with diaphragm flush at front. 2-wire system, process tempera- ture up to 140 deg. Cel., accuracy 0.2 % of f.s.v. output signal: 4...20 mA, Process connection: quick-release connection: connection o.cc.according DIN 11851 with slotted union nut: DN 25 Filling liquid: liquid FDA approved Output signal : 4-20 mA Housing(stainless steel1.4404)/ electrical connection: housing with angeld plug according DIN 43650, IP65 Measuring range: -1...3 bar overload pressure: 20 bar Without explosion protection ",463,"ΤΕΜ",1,"PI1",1,"7MF80101AD311FD1"]
["7MF8010-1AD31-1FE1","SITRANS P Transmitter Compact for pressure and absolut pressure for food, pharmaceu- ticals and biotechnology, with diaphragm flush at front. 2-wire system, process tempera- ture up to 140 deg. Cel., accuracy 0.2 % of f.s.v. output signal: 4...20 mA, Process connection: quick-release connection: connection o.cc.according DIN 11851 with slotted union nut: DN 25 Filling liquid: liquid FDA approved Output signal : 4-20 mA Housing(stainless steel1.4404)/ electrical connection: housing with angeld plug according DIN 43650, IP65 Measuring range: -1...5 bar overload pressure: 20 bar Without explosion protection ",463,"ΤΕΜ",1,"PI1",1,"7MF80101AD311FE1"]
["7NG3211-0NN00","Temperature transmitter SITRANS TH100 for PT100 for installation in connection head Type B (DIN 43729), two-wire system, 4...20 mA, programmable, without electrical isolation Without explosion protection . . ",92,"ΤΕΜ",1,"PI1",1,"7NG32110NN00"]
["7NG3211-0AN00","Temperature transmitter SITRANS TH100 for PT100 for installation in connection head Type B (DIN 43729), two-wire system, 4...20 mA, programmable, without electrical isolation With explosion protection Intrinsic safety and type of protection and zone 2 to ATEX . . ",133,"ΤΕΜ",1,"PI1",1,"7NG32110AN00"]
["7NG3211-1NN00","Temperature transmitter SITRANS TH200 for installation in connection head, type B (DIN 43729), two-wire system 4...20 mA, programmable, with electrical isolation Without explosion protection . . ",291,"ΤΕΜ",1,"PI1",1,"7NG32111NN00"]
["7NG3211-1AN00","Temperature transmitter SITRANS TH200 for installation in connection head, type B (DIN 43729), two-wire system 4...20 mA, programmable, with electrical isolation With explosion protection to ATEX . . ",353,"ΤΕΜ",1,"PI1",1,"7NG32111AN00"]
["7NG3212-0NN00","Temperature transmitter SITRANS TH300 For installation in the connection head, Type B (DIN 43729), Two-wire system 4 ... 20 mA, programmable, communication-capable acc. to HART, with electrical isolation Without explosion protection . . ",416,"ΤΕΜ",1,"PI1",1,"7NG32120NN00"]
["7NG3212-0AN00","Temperature transmitter SITRANS TH300 For installation in the connection head, Type B (DIN 43729), Two-wire system 4 ... 20 mA, programmable, communication-capable acc. to HART, with electrical isolation With explosion protection to ATEX . . ",480,"ΤΕΜ",1,"PI1",1,"7NG32120AN00"]
["7NG3092-8KN","Modem for SITRANS TH100/200 with USB interface and software SIPROM T ",277,"ΤΕΜ",1,"PI1",1,"7NG30928KN"]
["7NG3092-8KA","Adapter for rail mounting of head mounted transmitters (5 pcs.) ",81,"ΤΕΜ",1,"PI1",1,"7NG30928KA"]
["7NG3032-0JN00","Temperature transmitter SITRANS TR200, for rail mounting, 2-wire system, 4 to 20 mA, programmable, with galvanic isolation; with documentation on CD Without explosion protection . ",343,"ΤΕΜ",1,"PI1",1,"7NG30320JN00"]
["7NG3032-1JN00","Temperature transmitter SITRANS TR200, for rail mounting, 2-wire system, 4 to 20 mA, programmable, with galvanic isolation; with documentation on CD Explosion protection: with Eex ia . ",405,"ΤΕΜ",1,"PI1",1,"7NG30321JN00"]
["7NG3033-0JN00","Temperature transmitter SITRANS TR300, for mounting on a standard DIN rail, two-wire system, 4 ... 20 mA, HART, with electricial isolation, with documentation on CD Without explosion protection . . . ",462,"ΤΕΜ",1,"PI1",1,"7NG30330JN00"]
["7NG3033-1JN00","Temperature transmitter SITRANS TR300, for mounting on a standard DIN rail, two-wire system, 4 ... 20 mA, HART, with electricial isolation, with documentation on CD With explosion protection to ATEX . . . ",526,"ΤΕΜ",1,"PI1",1,"7NG30331JN00"]
["7NG3135-0AB10","SITRANS TF temperature trans- mitter in housing for field mounting, two-wire system 4 to 20mA, with electrical isolation, with documentation on DVD, integrated transmitter: SITRANS TH200, programmable; Without explosion protection Enclosure: Die-cast aluminium, Connections / Cable inlet screw gland M20 x 1,5; With digital indicator Without mounting bracket and securing parts; ",1151,"ΤΕΜ",1,"PI1",1,"7NG31350AB10"]
["7NG3135-1AB10","SITRANS TF temperature trans- mitter in housing for field mounting, two-wire system 4 to 20mA, with electrical isolation, with documentation on DVD, integrated transmitter: SITRANS TH200, programmable; Explosion protection: with Ex ia, Enclosure: Die-cast aluminium, Connections / Cable inlet screw gland M20 x 1,5; With digital indicator Without mounting bracket and securing parts; ",1206,"ΤΕΜ",1,"PI1",1,"7NG31351AB10"]
["7MC8005-5AA30-1BF0","Temperature sensor SITRANS TS300 for food, pharmaceuticals and biotechnology, modular design Head type: BS0; SS; threaded lid; IP67 Process connection: material 1.4404/316L milk pipe union to DIN 11851 with slotted union nut nominal diameter: DN 25, nominal pressure: PN 40 Protective tube: F1 = 9 mm Measuring insert: 6 mm, mineral insulated . Neck length: 80 mm Mounting length: 15 mm (0.59 inch) Sensor: 1 x Pt 100, class A, 3-wire . ",338,"ΤΕΜ",1,"PI1",1,"7MC80055AA301BF0"]
["7MC8005-5AA30-1CF0"," Temperature sensor SITRANS TS300 for food, pharmaceuticals and biotechnology, modular design Head type: BS0; SS; threaded lid; IP67 Process connection: material 1.4404/316L milk pipe union to DIN 11851 with slotted union nut nominal diameter: DN 25, nominal pressure: PN 40 Protective tube: F1 = 9 mm Measuring insert: 6 mm, mineral insulated . Neck length: 80 mm Mounting length: 16...35mm (0.63...1.38inch); Initial: 35mm(1.38inch) Sensor: 1 x Pt 100, class A, 3-wire .",338,"ΤΕΜ",1,"PI1",1,"7MC80055AA301CF0"]
["7MC8005-5AA30-1DF0"," Temperature sensor SITRANS TS300 for food, pharmaceuticals and biotechnology, modular design Head type: BS0; SS; threaded lid; IP67 Process connection: material 1.4404/316L milk pipe union to DIN 11851 with slotted union nut nominal diameter: DN 25, nominal pressure: PN 40 Protective tube: F1 = 9 mm Measuring insert: 6 mm, mineral insulated . Neck length: 80 mm Mounting length: 36...50mm (1.42...1.97inch); Initial: 50mm(1.97inch) Sensor: 1 x Pt 100, class A, 3-wire .",343,"ΤΕΜ",1,"PI1",1,"7MC80055AA301DF0"]
["7MC8005-5AA30-1EF0"," Temperature sensor SITRANS TS300 for food, pharmaceuticals and biotechnology, modular design Head type: BS0; SS; threaded lid; IP67 Process connection: material 1.4404/316L milk pipe union to DIN 11851 with slotted union nut nominal diameter: DN 25, nominal pressure: PN 40 Protective tube: F1 = 9 mm Measuring insert: 6 mm, mineral insulated . Neck length: 80 mm Mounting length: 51...100mm (2.01...3.94inch); Initial: 100mm(3.94inch) Sensor: 1 x Pt 100, class A, 3-wire .",344,"ΤΕΜ",1,"PI1",1,"7MC80055AA301EF0"]
["7MC8005-5AA30-1FF0"," Temperature sensor SITRANS TS300 for food, pharmaceuticals and biotechnology, modular design Head type: BS0; SS; threaded lid; IP67 Process connection: material 1.4404/316L milk pipe union to DIN 11851 with slotted union nut nominal diameter: DN 25, nominal pressure: PN 40 Protective tube: F1 = 9 mm Measuring insert: 6 mm, mineral insulated . Neck length: 80 mm Mounting length: 101...160mm (3.98...6.30inch); Initial: 160mm(6.30inch) Sensor: 1 x Pt 100, class A, 3-wire .",344,"ΤΕΜ",1,"PI1",1,"7MC80055AA301FF0"]
["7MC8005-5AA30-1GF0"," Temperature sensor SITRANS TS300 for food, pharmaceuticals and biotechnology, modular design Head type: BS0; SS; threaded lid; IP67 Process connection: material 1.4404/316L milk pipe union to DIN 11851 with slotted union nut nominal diameter: DN 25, nominal pressure: PN 40 Protective tube: F1 = 9 mm Measuring insert: 6 mm, mineral insulated . Neck length: 80 mm Mounting length: 161...250mm (6.34...9.84inch); Initial: 250mm(9.84inch) Sensor: 1 x Pt 100, class A, 3-wire .",345,"ΤΕΜ",1,"PI1",1,"7MC80055AA301GF0"]
["7MC8005-5AA30-1HF0"," Temperature sensor SITRANS TS300 for food, pharmaceuticals and biotechnology, modular design Head type: BS0; SS; threaded lid; IP67 Process connection: material 1.4404/316L milk pipe union to DIN 11851 with slotted union nut nominal diameter: DN 25, nominal pressure: PN 40 Protective tube: F1 = 9 mm Measuring insert: 6 mm, mineral insulated . Neck length: 80 mm Mounting length: 251...400mm (9.88...15.75inch); Initial: 400mm(15.75inch) Sensor: 1 x Pt 100, class A, 3-wire .",356,"ΤΕΜ",1,"PI1",1,"7MC80055AA301HF0"]
["7ME6910-1AA10-1AA0","MAG 5000, IP67 / NEMA 4X/6, Polyamid enclosure, With display, 115-230V AC 50/60 Hz ",1333,"ΤΕΜ",1,"PI2",1,"7ME69101AA101AA0"]
["7ME6910-1AA30-1AA0","MAG 5000, IP67 / NEMA 4X/6, Polyamid enclosure, With display, 11-30V DC/11-24V AC 50/60 Hz ",1333,"ΤΕΜ",1,"PI2",1,"7ME69101AA301AA0"]
["7ME6920-1AA10-1AA0","MAG 6000, IP67 / NEMA 4X/6, Polyamid enclosure, With display, 115-230V AC 50/60 Hz ",1569,"ΤΕΜ",1,"PI2",1,"7ME69201AA101AA0"]
["7ME6920-1AA30-1AA0","MAG 6000, IP67 / NEMA 4X/6, Polyamid enclosure, With display, 11-30V DC/11-24V AC 50/60 Hz ",1569,"ΤΕΜ",1,"PI2",1,"7ME69201AA301AA0"]
["FDK:085U1018","WALL MOUNTING UNIT, 4X M20 CABLE GLANDS",233,"ΤΕΜ",1,"PI2",1,"FDK:085U1018"]
["FDK:085U1053","Wall mounting unit, 4x 1/2 NPT cable glands",233,"ΤΕΜ",1,"PI2",1,"FDK:085U1053"]
["FDK:083F0121","SITRANS F M Accessory MAG 5000/6000 10 m (32.8 ft) Standard coil or electrode cable, 3x 1.5 mm2 (3x 0.0024 inch2), gage 18, single shielded with PVC jacket, temperature range: -30…+70 °C (-22…+ 158 °F) ",57,"ΤΕΜ",1,"PI2",1,"FDK:083F0121"]
["FDK:083F0210","SITRANS F M Accessory MAG 5000/6000 20 m (65.6 ft) Standard coil or electrode cable, 3x 1.5 mm2 (3x 0.0024 inch2), gage 18, single shielded with PVC jacket, temperature range: -30…+70 °C (-22…+ 158 °F) ",116,"ΤΕΜ",1,"PI2",1,"FDK:083F0210"]
["FDK:083F0211","SITRANS F M Accessory MAG 5000/6000 40 m (131.2 ft) Standard coil or electrode cable, 3x 1.5 mm2 (3x 0.0024 inch2), gage 18, single shielded with PVC jacket, temperature range: -30…+70 °C (-22…+ 158 °F) ",230,"ΤΕΜ",1,"PI2",1,"FDK:083F0211"]
["FDK:083F0212","SITRANS F M Accessory MAG 5000/6000 60 m (196.9 ft) Standard coil or electrode cable, 3x 1.5 mm2 (3x 0.0024 inch2), gage 18, single shielded with PVC jacket, temperature range: -30…+70 °C (-22…+ 158 °F) ",343,"ΤΕΜ",1,"PI2",1,"FDK:083F0212"]
["A5E02296329","SITRANS F M Accessory MAG 5000/6000 2x 5 m (16.4 ft) Cable kit including standard coil cable, 3x 1.5 mm2 (3x 0.0024 inch2), gage 18, single shielded with PVC jacket, and special electrode cable, 3x 0.25 mm2 (3x 0.0004 inch2), double shielded with PVC jacket, temperature range: -30 … +70 °C (-22 °F … +158 °F) ",111,"ΤΕΜ",1,"PI2",1,"A5E02296329"]
["A5E01181647","SITRANS F M Accessory MAG 5000/6000 2x 10 m (32.8 ft) Cable kit including standard coil cable, 3x 1.5 mm2 (3x 0.0024 inch2), gage 18, single shielded with PVC jacket, and special electrode cable, 3x 0.25 mm2 (3x 0.0004 inch2), double shielded with PVC jacket, temperature range: -30 … +70 °C (-22 °F … +158 °F) ",179,"ΤΕΜ",1,"PI2",1,"A5E01181647"]
["A5E02296464","SITRANS F M Accessory MAG 5000/6000 2x 15 m (49.2 ft) Cable kit including standard coil cable, 3x 1.5 mm2 (3x 0.0024 inch2), gage 18, single shielded with PVC jacket, and special electrode cable, 3x 0.25 mm2 (3x 0.0004 inch2), double shielded with PVC jacket, temperature range: -30 … +70 °C (-22 °F … +158 °F) ",311,"ΤΕΜ",1,"PI2",1,"A5E02296464"]
["A5E01181656","SITRANS F M Accessory MAG 5000/6000 2x 20 m (65.6 ft) Cable kit including standard coil cable, 3x 1.5 mm2 (3x 0.0024 inch2), gage 18, single shielded with PVC jacket, and special electrode cable, 3x 0.25 mm2 (3x 0.0004 inch2), double shielded with PVC jacket, temperature range: -30â€¦+70 Â°C (-22â€¦+ 158 Â°F) ",331,"ΤΕΜ",1,"PI2",1,"A5E01181656"]
["A5E02296490","SITRANS F M Accessory MAG 5000/6000 2x 25 m (82.0 ft) Cable kit including standard coil cable, 3x 1.5 mm2 (3x 0.0024 inch2), gage 18, single shielded with PVC jacket, and special electrode cable, 3x 0.25 mm2 (3x 0.0004 inch2), double shielded with PVC jacket, temperature range: -30 … +70 °C (-22 °F … +158 °F) ",416,"ΤΕΜ",1,"PI2",1,"A5E02296490"]
["A5E01181686","SITRANS F M Accessory MAG 5000/6000 2x 40 m (131.2 ft) Cable kit including standard coil cable, 3x 1.5 mm2 (3x 0.0024 inch2), gage 18, single shielded with PVC jacket, and special electrode cable, 3x 0.25 mm2 (3x 0.0004 inch2), double shielded with PVC jacket, temperature range: -30 … +70 °C (-22 °F … +158 °F) ",650,"ΤΕΜ",1,"PI2",1,"A5E01181686"]
["A5E01181691","SITRANS F M Accessory MAG 5000/6000 2x 100 m (328.1 ft) Cable kit including standard coil cable, 3x 1.5 mm2 (3x 0.0024 inch2), gage 18, single shielded with PVC jacket, and special electrode cable, 3x 0.25 mm2 (3x 0.0004 inch2), double shielded with PVC jacket, temperature range: -30 … +70 °C (-22 °F … +158 °F) ",1739,"ΤΕΜ",1,"PI2",1,"A5E01181691"]
["A5E01181699","SITRANS F M Accessory MAG 5000/6000 2x 150 m (491.1 ft) Cable kit including standard coil cable, 3x 1.5 mm2 (3x 0.0024 inch2), gage 18, single shielded with PVC jacket, and special electrode cable, 3x 0.25 mm2 (3x 0.0004 inch2), double shielded with PVC jacket, temperature range: -30 … +70 °C (-22 °F … +158 °F) ",2507,"ΤΕΜ",1,"PI2",1,"A5E01181699"]
["A5E02328485","Accessories, Suncover",49,"ΤΕΜ",1,"PI2",1,"A5E02328485"]
["FDK:085U0220","USM Potting Kit",142,"ΤΕΜ",1,"PI2",1,"FDK:085U0220"]
["FDK:085U0226","USM II, HART MODUL",220,"ΤΕΜ",1,"PI2",1,"FDK:085U0226"]
["FDK:085U0234","USM II, MODBUS RTU modul",220,"ΤΕΜ",1,"PI2",1,"FDK:085U0234"]
["FDK:085U0236","Add-on module Profibus PA profile 3.",452,"ΤΕΜ",1,"PI2",1,"FDK:085U0236"]
["FDK:085U0237","Add-on module Profibus DP profile 3.",452,"ΤΕΜ",1,"PI2",1,"FDK:085U0237"]
["7ME6140-1RB10-1AA1"," SITRANS FM MAG 1100 F Full-bore electromagnetic flow sensor, sanitary design, diameter DN 10 to DN 100 (3/8\" to 4\"). Suitable for volume flow measurement of liquids (conductive) , for applications in F&B, pharmaceutical industry. . DN10, 3/8 Inch Weld in connection fittings: DIN11850 PFA (no ATEX) EPDM (FDA) Electrode material: Hastelloy C Sensor for remote transmitter (order transmitter separately)- 3A approved No bus Communication Metric Polyamid terminal box (3A) or 6000 I compact.",1721,"ΤΕΜ",1,"PI2",1,"7ME61401RB101AA1"]
["7ME6140-1VB10-1AA1"," SITRANS FM MAG 1100 F Full-bore electromagnetic flow sensor, sanitary design, diameter DN 10 to DN 100 (3/8\" to 4\"). Suitable for volume flow measurement of liquids (conductive) , for applications in F&B, pharmaceutical industry. . DN15, 1/2 Inch Weld in connection fittings: DIN11850 PFA (no ATEX) EPDM (FDA) Electrode material: Hastelloy C Sensor for remote transmitter (order transmitter separately)- 3A approved No bus Communication Metric Polyamid terminal box (3A) or 6000 I compact.",1721,"ΤΕΜ",1,"PI2",1,"7ME61401VB101AA1"]
["7ME6140-2DB10-1AA1"," SITRANS FM MAG 1100 F Full-bore electromagnetic flow sensor, sanitary design, diameter DN 10 to DN 100 (3/8\" to 4\"). Suitable for volume flow measurement of liquids (conductive) , for applications in F&B, pharmaceutical industry. . DN25, 1 Inch Weld in connection fittings: DIN11850 PFA (no ATEX) EPDM (FDA) Electrode material: Hastelloy C Sensor for remote transmitter (order transmitter separately)- 3A approved No bus Communication Metric Polyamid terminal box (3A) or 6000 I compact.",1763,"ΤΕΜ",1,"PI2",1,"7ME61402DB101AA1"]
["7ME6140-2RB10-1AA1"," SITRANS FM MAG 1100 F Full-bore electromagnetic flow sensor, sanitary design, diameter DN 10 to DN 100 (3/8\" to 4\"). Suitable for volume flow measurement of liquids (conductive) , for applications in F&B, pharmaceutical industry. . DN40, 1 1/2 Inch Weld in connection fittings: DIN11850 PFA (no ATEX) EPDM (FDA) Electrode material: Hastelloy C Sensor for remote transmitter (order transmitter separately)- 3A approved No bus Communication Metric Polyamid terminal box (3A) or 6000 I compact.",2084,"ΤΕΜ",1,"PI2",1,"7ME61402RB101AA1"]
["7ME6140-2YB10-1AA1"," SITRANS FM MAG 1100 F Full-bore electromagnetic flow sensor, sanitary design, diameter DN 10 to DN 100 (3/8\" to 4\"). Suitable for volume flow measurement of liquids (conductive) , for applications in F&B, pharmaceutical industry. . DN50, 2 Inch Weld in connection fittings: DIN11850 PFA (no ATEX) EPDM (FDA) Electrode material: Hastelloy C Sensor for remote transmitter (order transmitter separately)- 3A approved No bus Communication Metric Polyamid terminal box (3A) or 6000 I compact.",2380,"ΤΕΜ",1,"PI2",1,"7ME61402YB101AA1"]
["7ME6140-3FB10-1AA1"," SITRANS FM MAG 1100 F Full-bore electromagnetic flow sensor, sanitary design, diameter DN 10 to DN 100 (3/8\" to 4\"). Suitable for volume flow measurement of liquids (conductive) , for applications in F&B, pharmaceutical industry. . DN65, 2 1/2 Inch Weld in connection fittings: DIN11850 PFA (no ATEX) EPDM (FDA) Electrode material: Hastelloy C Sensor for remote transmitter (order transmitter separately)- 3A approved No bus Communication Metric Polyamid terminal box (3A) or 6000 I compact.",2531,"ΤΕΜ",1,"PI2",1,"7ME61403FB101AA1"]
["7ME6140-3MB10-1AA1"," SITRANS FM MAG 1100 F Full-bore electromagnetic flow sensor, sanitary design, diameter DN 10 to DN 100 (3/8\" to 4\"). Suitable for volume flow measurement of liquids (conductive) , for applications in F&B, pharmaceutical industry. . DN80, 3 Inch Weld in connection fittings: DIN11850 PFA (no ATEX) EPDM (FDA) Electrode material: Hastelloy C Sensor for remote transmitter (order transmitter separately)- 3A approved No bus Communication Metric Polyamid terminal box (3A) or 6000 I compact.",2724,"ΤΕΜ",1,"PI2",1,"7ME61403MB101AA1"]
["7ME6140-3TB10-1AA1"," SITRANS FM MAG 1100 F Full-bore electromagnetic flow sensor, sanitary design, diameter DN 10 to DN 100 (3/8\" to 4\"). Suitable for volume flow measurement of liquids (conductive) , for applications in F&B, pharmaceutical industry. . DN100, 4 Inch Weld in connection fittings: DIN11850 PFA (no ATEX) EPDM (FDA) Electrode material: Hastelloy C Sensor for remote transmitter (order transmitter separately)- 3A approved No bus Communication Metric Polyamid terminal box (3A) or 6000 I compact.",3259,"ΤΕΜ",1,"PI2",1,"7ME61403TB101AA1"]
["7ME6520-2DF13-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN25, 1 Inch EN 1092-1, PN 40 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",1082,"ΤΕΜ",1,"PI2",1,"7ME65202DF132AA1"]
["7ME6520-2RF13-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN40, 1 1/2 Inch EN 1092-1, PN 40 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",1097,"ΤΕΜ",1,"PI2",1,"7ME65202RF132AA1"]
["7ME6520-2YC13-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN50, 2 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",1132,"ΤΕΜ",1,"PI2",1,"7ME65202YC132AA1"]
["7ME6520-3FC13-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN65, 2 1/2 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",1144,"ΤΕΜ",1,"PI2",1,"7ME65203FC132AA1"]
["7ME6520-3MC13-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN80, 3 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",1155,"ΤΕΜ",1,"PI2",1,"7ME65203MC132AA1"]
["7ME6520-3TC13-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN100, 4 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",1206,"ΤΕΜ",1,"PI2",1,"7ME65203TC132AA1"]
["7ME6520-4BC13-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN125, 5 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",1417,"ΤΕΜ",1,"PI2",1,"7ME65204BC132AA1"]
["7ME6520-4HC13-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN150, 6 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",1609,"ΤΕΜ",1,"PI2",1,"7ME65204HC132AA1"]
["7ME6520-4PB13-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN200, 8 Inch EN 1092-1, PN 10 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",1870,"ΤΕΜ",1,"PI2",1,"7ME65204PB132AA1"]
["7ME6520-4PC13-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN200, 8 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",1935,"ΤΕΜ",1,"PI2",1,"7ME65204PC132AA1"]
["7ME6520-4VB13-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN250, 10 Inch EN 1092-1, PN 10 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",2313,"ΤΕΜ",1,"PI2",1,"7ME65204VB132AA1"]
["7ME6520-4VC13-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN250, 10 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",2425,"ΤΕΜ",1,"PI2",1,"7ME65204VC132AA1"]
["7ME6520-5DB13-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN300, 12 Inch EN 1092-1, PN 10 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",3434,"ΤΕΜ",1,"PI2",1,"7ME65205DB132AA1"]
["7ME6520-5DC13-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN300, 12 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",3610,"ΤΕΜ",1,"PI2",1,"7ME65205DC132AA1"]
["7ME6520-5KB13-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN350, 14 Inch EN 1092-1, PN 10 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",4740,"ΤΕΜ",1,"PI2",1,"7ME65205KB132AA1"]
["7ME6520-5KC13-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN350, 14 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",4952,"ΤΕΜ",1,"PI2",1,"7ME65205KC132AA1"]
["7ME6520-5RB13-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN400, 16 Inch EN 1092-1, PN 10 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",5258,"ΤΕΜ",1,"PI2",1,"7ME65205RB132AA1"]
["7ME6520-5RC13-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN400, 16 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",5533,"ΤΕΜ",1,"PI2",1,"7ME65205RC132AA1"]
["7ME6520-5YB13-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN450, 18 Inch EN 1092-1, PN 10 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",5767,"ΤΕΜ",1,"PI2",1,"7ME65205YB132AA1"]
["7ME6520-5YC13-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN450, 18 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",6450,"ΤΕΜ",1,"PI2",1,"7ME65205YC132AA1"]
["7ME6520-6FB13-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN500, 20 Inch EN 1092-1, PN 10 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",6277,"ΤΕΜ",1,"PI2",1,"7ME65206FB132AA1"]
["7ME6520-6FC13-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN500, 20 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",7163,"ΤΕΜ",1,"PI2",1,"7ME65206FC132AA1"]
["7ME6520-6PB13-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN600, 24 Inch EN 1092-1, PN 10 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",6984,"ΤΕΜ",1,"PI2",1,"7ME65206PB132AA1"]
["7ME6520-6PC13-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN600, 24 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: Hard NBR Rubber Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",7950,"ΤΕΜ",1,"PI2",1,"7ME65206PC132AA1"]
["7ME6520-2DF12-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN25, 1 Inch EN 1092-1, PN 40 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",1138,"ΤΕΜ",1,"PI2",1,"7ME65202DF122AA1"]
["7ME6520-2RF12-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN40, 1 1/2 Inch EN 1092-1, PN 40 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",1149,"ΤΕΜ",1,"PI2",1,"7ME65202RF122AA1"]
["7ME6520-2YC12-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN50, 2 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",1187,"ΤΕΜ",1,"PI2",1,"7ME65202YC122AA1"]
["7ME6520-3FC12-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN65, 2 1/2 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",1202,"ΤΕΜ",1,"PI2",1,"7ME65203FC122AA1"]
["7ME6520-3MC12-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN80, 3 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",1215,"ΤΕΜ",1,"PI2",1,"7ME65203MC122AA1"]
["7ME6520-3TC12-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN100, 4 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",1268,"ΤΕΜ",1,"PI2",1,"7ME65203TC122AA1"]
["7ME6520-4BC12-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN125, 5 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",1490,"ΤΕΜ",1,"PI2",1,"7ME65204BC122AA1"]
["7ME6520-4HC12-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN150, 6 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",1689,"ΤΕΜ",1,"PI2",1,"7ME65204HC122AA1"]
["7ME6520-4PB12-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN200, 8 Inch EN 1092-1, PN 10 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",1962,"ΤΕΜ",1,"PI2",1,"7ME65204PB122AA1"]
["7ME6520-4PC12-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN200, 8 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",2034,"ΤΕΜ",1,"PI2",1,"7ME65204PC122AA1"]
["7ME6520-4VB12-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN250, 10 Inch EN 1092-1, PN 10 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",2428,"ΤΕΜ",1,"PI2",1,"7ME65204VB122AA1"]
["7ME6520-4VC12-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN250, 10 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",2545,"ΤΕΜ",1,"PI2",1,"7ME65204VC122AA1"]
["7ME6520-5DB12-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN300, 12 Inch EN 1092-1, PN 10 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",3604,"ΤΕΜ",1,"PI2",1,"7ME65205DB122AA1"]
["7ME6520-5DC12-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN300, 12 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",3794,"ΤΕΜ",1,"PI2",1,"7ME65205DC122AA1"]
["7ME6520-5KB12-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN350, 14 Inch EN 1092-1, PN 10 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",4974,"ΤΕΜ",1,"PI2",1,"7ME65205KB122AA1"]
["7ME6520-5KC12-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN350, 14 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",5199,"ΤΕΜ",1,"PI2",1,"7ME65205KC122AA1"]
["7ME6520-5RB12-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN400, 16 Inch EN 1092-1, PN 10 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",5523,"ΤΕΜ",1,"PI2",1,"7ME65205RB122AA1"]
["7ME6520-5RC12-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN400, 16 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",5812,"ΤΕΜ",1,"PI2",1,"7ME65205RC122AA1"]
["7ME6520-5YB12-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN450, 18 Inch EN 1092-1, PN 10 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",6054,"ΤΕΜ",1,"PI2",1,"7ME65205YB122AA1"]
["7ME6520-5YC12-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN450, 18 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",6457,"ΤΕΜ",1,"PI2",1,"7ME65205YC122AA1"]
["7ME6520-6FB12-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN500, 20 Inch EN 1092-1, PN 10 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",6591,"ΤΕΜ",1,"PI2",1,"7ME65206FB122AA1"]
["7ME6520-6FC12-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN500, 20 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",7174,"ΤΕΜ",1,"PI2",1,"7ME65206FC122AA1"]
["7ME6520-6PB12-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN600, 24 Inch EN 1092-1, PN 10 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",7334,"ΤΕΜ",1,"PI2",1,"7ME65206PB122AA1"]
["7ME6520-6PC12-2AA1"," SITRANS FM MAG 5100 W Electromagnetic flow sensor, flanged, diameter DN 15 to DN 1200 (1/2\" to 48\"). Suitable for volume flow measurement of liquids (conductive) , for applications in water abstraction, water & wastewater treatment, water distribution networks, custody transfer metering. . DN600, 24 Inch EN 1092-1, PN 16 Carbon steel flanges ASTM A 105, corrosion-resistant coating of category C4 Liner Material: EPDM Hastelloy C-276 Sensor for remote transmitter (order transmitter separately) No bus communication Metric Polyamid terminal box or 6000 I compact.",7963,"ΤΕΜ",1,"PI2",1,"7ME65206PC122AA1"]
["7ME6810-2DF31-1AA1"," SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN25 / Qmx 17 m3/h(m3), 1 Inch / Qmx 74 GPM(G), DN25 / Qmx 0.408 Ml/d(Ml) EN1092-1, PN40, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor No additional communication, Standard IrDA interface Internal 2 D-cell battery pack installed and disconnected inside meter",2938,"ΤΕΜ",1,"PI1",1,"7ME68102DF311AA1"]
["7ME6810-2RF31-1AA1"," SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN40 / Qmx 45 m3/h(m3), 1 1/2 Inch / Qmx 198 GPM(G), DN40 / Qmx 1.08 Ml/d(Ml) EN1092-1, PN40, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor No additional communication, Standard IrDA interface Internal 2 D-cell battery pack installed and disconnected inside meter",2953,"ΤΕΜ",1,"PI1",1,"7ME68102RF311AA1"]
["7ME6810-2YC31-1AA1"," SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN50 / Qmx 63 m3/h(m3), 2 Inch / Qmx 277 GPM(G), DN50 / Qmx 1.512 Ml/d(Ml) EN 1092-1, PN 16, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor No additional communication, Standard IrDA interface Internal 2 D-cell battery pack installed and disconnected inside meter",2988,"ΤΕΜ",1,"PI1",1,"7ME68102YC311AA1"]
["7ME6810-3FC31-1AA1"," SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN65 / Qmx 100 m3/h(m3), 2 1/2 Inch / Qmx 440 GPM(G), DN65 / Qmx 2.4 Ml/d(Ml) EN 1092-1, PN 16, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor No additional communication, Standard IrDA interface Internal 2 D-cell battery pack installed and disconnected inside meter",3000,"ΤΕΜ",1,"PI1",1,"7ME68103FC311AA1"]
["7ME6810-3MC31-1AA1"," SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN80 / Qmx 160 m3/h(m3), 3 Inch / Qmx 704 GPM(Gx100), DN80 / Qmx 3.84 Ml/d(Ml) EN 1092-1, PN 16, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor No additional communication, Standard IrDA interface Internal 2 D-cell battery pack installed and disconnected inside meter",3011,"ΤΕΜ",1,"PI1",1,"7ME68103MC311AA1"]
["7ME6810-3TC31-1AA1"," SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN100 / Qmx 250 m3/h(m3), 4 Inch / Qmx 1100 GPM(Gx100) , DN100 / Qmx 6 Ml/d(Ml) EN 1092-1, PN 16, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor No additional communication, Standard IrDA interface Internal 2 D-cell battery pack installed and disconnected inside meter",3062,"ΤΕΜ",1,"PI1",1,"7ME68103TC311AA1"]
["7ME6810-4BC31-1AA1"," SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN125 / Qmx 400 m3/h(m3), 5 Inch / Qmx 1761 GPM(Gx100) , DN125 / Qmx 9.6 Ml/d(Ml) EN 1092-1, PN 16, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor No additional communication, Standard IrDA interface Internal 2 D-cell battery pack installed and disconnected inside meter",3273,"ΤΕΜ",1,"PI1",1,"7ME68104BC311AA1"]
["7ME6810-4HC31-1AA1"," SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN150 / Qmx 629 m3/h(m3), 6 Inch / Qmx 2769 GPM(Gx100) , DN150 / Qmx 15.12 Ml/d(Ml) EN 1092-1, PN 16, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor No additional communication, Standard IrDA interface Internal 2 D-cell battery pack installed and disconnected inside meter",3466,"ΤΕΜ",1,"PI1",1,"7ME68104HC311AA1"]
["7ME6810-4PB31-1AA1"," SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN200 / Qmx 997 m3/h(m3), 8 Inch / Qmx 4389 GPM(Gx100) , DN200 / Qmx 24 Ml/d(Ml) EN 1092-1, PN 10, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor No additional communication, Standard IrDA interface Internal 2 D-cell battery pack installed and disconnected inside meter",3727,"ΤΕΜ",1,"PI1",1,"7ME68104PB311AA1"]
["7ME6810-4PC31-1AA1"," SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN200 / Qmx 997 m3/h(m3), 8 Inch / Qmx 4389 GPM(Gx100) , DN200 / Qmx 24 Ml/d(Ml) EN 1092-1, PN 16, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor No additional communication, Standard IrDA interface Internal 2 D-cell battery pack installed and disconnected inside meter",3791,"ΤΕΜ",1,"PI1",1,"7ME68104PC311AA1"]
["7ME6810-4VB31-1AA1"," SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN250 / Qmx 1600 m3/h(m3), 10 Inch / Qmx 7044 GPM(Gx10 0), 250 / Qmx 38.4 Ml/d(Ml) EN 1092-1, PN 10, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor No additional communication, Standard IrDA interface Internal 2 D-cell battery pack installed and disconnected inside meter",4170,"ΤΕΜ",1,"PI1",1,"7ME68104VB311AA1"]
["7ME6810-4VC31-1AA1"," SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN250 / Qmx 1600 m3/h(m3), 10 Inch / Qmx 7044 GPM(Gx10 0), 250 / Qmx 38.4 Ml/d(Ml) EN 1092-1, PN 16, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor No additional communication, Standard IrDA interface Internal 2 D-cell battery pack installed and disconnected inside meter",4281,"ΤΕΜ",1,"PI1",1,"7ME68104VC311AA1"]
["7ME6810-5DB31-1AA1"," SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN300 / Qmx 2500 m3/h(m3), 12 Inch / Qmx 11007 GPM(Gx10 0), 300 / Qmx 60 Ml/d(Ml) EN 1092-1, PN 10, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor No additional communication, Standard IrDA interface Internal 2 D-cell battery pack installed and disconnected inside meter",5290,"ΤΕΜ",1,"PI1",1,"7ME68105DB311AA1"]
["7ME6810-5DC31-1AA1"," SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN300 / Qmx 2500 m3/h(m3), 12 Inch / Qmx 11007 GPM(Gx10 0), 300 / Qmx 60 Ml/d(Ml) EN 1092-1, PN 16, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor No additional communication, Standard IrDA interface Internal 2 D-cell battery pack installed and disconnected inside meter",5467,"ΤΕΜ",1,"PI1",1,"7ME68105DC311AA1"]
["7ME6810-5KB31-1AA1"," SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN350 / Qmx 3463 m3/h(m3), 14 Inch / Qmx 15247 GPM(Gx100 0), 350 / Qmx 83.11 Ml/d(Ml) EN 1092-1, PN 10, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor No additional communication, Standard IrDA interface Internal 2 D-cell battery pack installed and disconnected inside meter",7578,"ΤΕΜ",1,"PI1",1,"7ME68105KB311AA1"]
["7ME6810-5KC31-1AA1"," SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN350 / Qmx 3463 m3/h(m3), 14 Inch / Qmx 15247 GPM(Gx100 0), 350 / Qmx 83.11 Ml/d(Ml) EN 1092-1, PN 16, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor No additional communication, Standard IrDA interface Internal 2 D-cell battery pack installed and disconnected inside meter",7810,"ΤΕΜ",1,"PI1",1,"7ME68105KC311AA1"]
["7ME6810-5RB31-1AA1"," SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN400 / Qmx 4523 m3/h(m3), 16 Inch / Qmx 19914 GPM(Gx100 0), 400 / Qmx 108.5 Ml/d(Ml) EN 1092-1, PN 10, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor No additional communication, Standard IrDA interface Internal 2 D-cell battery pack installed and disconnected inside meter",9139,"ΤΕΜ",1,"PI1",1,"7ME68105RB311AA1"]
["7ME6810-5RC31-1AA1"," SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN400 / Qmx 4523 m3/h(m3), 16 Inch / Qmx 19914 GPM(Gx100 0), 400 / Qmx 108.5 Ml/d(Ml) EN 1092-1, PN 16, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor No additional communication, Standard IrDA interface Internal 2 D-cell battery pack installed and disconnected inside meter",9461,"ΤΕΜ",1,"PI1",1,"7ME68105RC311AA1"]
["7ME6810-5YB31-1AA1"," SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN450 / Qmx 5725 m3/h(m3), 18 Inch / Qmx 25207 GPM(Gx100 0), 450 / Qmx 137.4 Ml/d(Ml) EN 1092-1, PN 10, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor No additional communication, Standard IrDA interface Internal 2 D-cell battery pack installed and disconnected inside meter",10157,"ΤΕΜ",1,"PI1",1,"7ME68105YB311AA1"]
["7ME6810-5YC31-1AA1"," SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN450 / Qmx 5725 m3/h(m3), 18 Inch / Qmx 25207 GPM(Gx100 0), 450 / Qmx 137.4 Ml/d(Ml) EN 1092-1, PN 16, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor No additional communication, Standard IrDA interface Internal 2 D-cell battery pack installed and disconnected inside meter",10560,"ΤΕΜ",1,"PI1",1,"7ME68105YC311AA1"]
["7ME6810-6FB31-1AA1"," SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN500 / Qmx 7068 m3/h(m3), 20 Inch / Qmx 31120 GPM(Gx100 0), 500 / Qmx 169.6 Ml/d(Ml) EN 1092-1, PN 10, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor No additional communication, Standard IrDA interface Internal 2 D-cell battery pack installed and disconnected inside meter",11825,"ΤΕΜ",1,"PI1",1,"7ME68106FB311AA1"]
["7ME6810-6FC31-1AA1"," SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN500 / Qmx 7068 m3/h(m3), 20 Inch / Qmx 31120 GPM(Gx100 0), 500 / Qmx 169.6 Ml/d(Ml) EN 1092-1, PN 16, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor No additional communication, Standard IrDA interface Internal 2 D-cell battery pack installed and disconnected inside meter",12503,"ΤΕΜ",1,"PI1",1,"7ME68106FC311AA1"]
["7ME6810-6PB31-1AA1"," SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN600 / Qmx 10178 m3/h(m3), 24 Inch / Qmx 44813 GPM(Gx100 0), 600 / Qmx 244.2 Ml/d(Ml) EN 1092-1, PN 10, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor No additional communication, Standard IrDA interface Internal 2 D-cell battery pack installed and disconnected inside meter",13881,"ΤΕΜ",1,"PI1",1,"7ME68106PB311AA1"]
["7ME6810-6PC31-1AA1"," SITRANS FM MAG 8000 Battery-operated electromagnetic flowmeter, flanged, diameter DN 25 to DN 1200 (1\" to 48\"). Suitable for volume flow measurement of liquids (conductive) and water applications within abstraction, distribution network, revenue metering and irrigation. . DN600 / Qmx 10178 m3/h(m3), 24 Inch / Qmx 44813 GPM(Gx100 0), 600 / Qmx 244.2 Ml/d(Ml) EN 1092-1, PN 16, Conforms to PED EPDM liner and Hastelloy Electrodes, corrosion-resistant coating of category C4 Standard calibration w. max. 0,4% of rate +/- 2mm/s with certificate Region version: Europe Display: m3 based 50 Hz filter Basic version compact Transmitter on sensor No additional communication, Standard IrDA interface Internal 2 D-cell battery pack installed and disconnected inside meter",14615,"ΤΕΜ",1,"PI1",1,"7ME68106PC311AA1"]
["FDK:087L4163","MAG8000 Accessories USB Irda adapter",218,"ΤΕΜ",1,"PI1",1,"FDK:087L4163"]
["7ML5501-0EA10","Pointek CLS100 RF Capacitance point level switch, stainless steel process connection. Detects level and interface in liquids, solids, slurries and foam. Compact, with 100 mm (4 inch) insertion, adaptable sensitivity, with the ability to tune out build-up on probe. . . Process connection: R 1\" ((BSPT), EN 10226/PT (JIS-T), JIS B 0203) Approvals: general purpose Device version: Integral cable version (PPS probe) Overfill Protection: Not required ",297,"ΤΕΜ",1,"PI3",1,"7ML55010EA10"]
["7ML5501-0EC10","Pointek CLS100 RF Capacitance point level switch, stainless steel process connection. Detects level and interface in liquids, solids, slurries and foam. Compact, with 100 mm (4 inch) insertion, adaptable sensitivity, with the ability to tune out build-up on probe. . . Process connection: R 1\" ((BSPT), EN 10226/PT (JIS-T), JIS B 0203) Approval: CSA/FM Class I, II and III, Div. 1, Groups A, B, C, D, E, F, G T4; ATEX II 1 GD 1/2GD EEx ia IIC T4 to T6 T107 'C Device version: Integral cable version (PPS probe) Overfill Protection: Not required ",379,"ΤΕΜ",1,"PI3",1,"7ML55010EC10"]
["7ML5501-0EA30","Pointek CLS100 RF Capacitance point level switch, stainless steel process connection. Detects level and interface in liquids, solids, slurries and foam. Compact, with 100 mm (4 inch) insertion, adaptable sensitivity, with the ability to tune out build-up on probe. . . Process connection: R 1\" ((BSPT), EN 10226/PT (JIS-T), JIS B 0203) Approvals: general purpose Device version: Enclosure version (PPS probe), 1/2 \" NPT cable inlet Overfill Protection: Not required ",357,"ΤΕΜ",1,"PI3",1,"7ML55010EA30"]
["7ML5501-0EC30","Pointek CLS100 RF Capacitance point level switch, stainless steel process connection. Detects level and interface in liquids, solids, slurries and foam. Compact, with 100 mm (4 inch) insertion, adaptable sensitivity, with the ability to tune out build-up on probe. . . Process connection: R 1\" ((BSPT), EN 10226/PT (JIS-T), JIS B 0203) Approval: CSA/FM Class I, II and III, Div. 1, Groups A, B, C, D, E, F, G T4; ATEX II 1 GD 1/2GD EEx ia IIC T4 to T6 T107 'C Device version: Enclosure version (PPS probe), 1/2 \" NPT cable inlet Overfill Protection: Not required ",438,"ΤΕΜ",1,"PI3",1,"7ML55010EC30"]
["7ML5501-0EA60","Pointek CLS100 RF Capacitance point level switch, stainless steel process connection. Detects level and interface in liquids, solids, slurries and foam. Compact, with 100 mm (4 inch) insertion, adaptable sensitivity, with the ability to tune out build-up on probe. . . Process connection: R 1\" ((BSPT), EN 10226/PT (JIS-T), JIS B 0203) Approvals: general purpose Device version: Enclosure version with PVDF probe body, (1/2\" NPT cable inlet) Overfill Protection: Not required ",455,"ΤΕΜ",1,"PI3",1,"7ML55010EA60"]
["7ML5501-0EC60","Pointek CLS100 RF Capacitance point level switch, stainless steel process connection. Detects level and interface in liquids, solids, slurries and foam. Compact, with 100 mm (4 inch) insertion, adaptable sensitivity, with the ability to tune out build-up on probe. . . Process connection: R 1\" ((BSPT), EN 10226/PT (JIS-T), JIS B 0203) Approval: CSA/FM Class I, II and III, Div. 1, Groups A, B, C, D, E, F, G T4; ATEX II 1 GD 1/2GD EEx ia IIC T4 to T6 T107 'C Device version: Enclosure version with PVDF probe body, (1/2\" NPT cable inlet) Overfill Protection: Not required ",537,"ΤΕΜ",1,"PI3",1,"7ML55010EC60"]
["7ML5501-0EA70","Pointek CLS100 RF Capacitance point level switch, stainless steel process connection. Detects level and interface in liquids, solids, slurries and foam. Compact, with 100 mm (4 inch) insertion, adaptable sensitivity, with the ability to tune out build-up on probe. . . Process connection: R 1\" ((BSPT), EN 10226/PT (JIS-T), JIS B 0203) Approvals: general purpose Device version: Enclosure version (PPS probe), M20x1.5 cable inlet Overfill Protection: Not required ",376,"ΤΕΜ",1,"PI3",1,"7ML55010EA70"]
["7ML5501-0EC70","Pointek CLS100 RF Capacitance point level switch, stainless steel process connection. Detects level and interface in liquids, solids, slurries and foam. Compact, with 100 mm (4 inch) insertion, adaptable sensitivity, with the ability to tune out build-up on probe. . . Process connection: R 1\" ((BSPT), EN 10226/PT (JIS-T), JIS B 0203) Approval: CSA/FM Class I, II and III, Div. 1, Groups A, B, C, D, E, F, G T4; ATEX II 1 GD 1/2GD EEx ia IIC T4 to T6 T107 'C Device version: Enclosure version (PPS probe), M20x1.5 cable inlet Overfill Protection: Not required ",458,"ΤΕΜ",1,"PI3",1,"7ML55010EC70"]
["7ML5610-0BD10","Pointek CLS100 RF Capacitance point level switch, PPS process connection. Detects level and interface in liquids, solids, slurries, and foam. Compact, with 100 mm (4 inch) insertion, adaptable sensitivity, with the ability to tune out build-up on probe. . Process connection: R 1\" ((BSPT), EN 10226/PT (JIS-T), JIS B 0203) (PPS probe body) Approvals: General Purpose (CSA, FM) Versions/Options: Enclosure version, PPS process connection, 1/2 inch NPT cable inlet Overfill Protection: Not Required ",267,"ΤΕΜ",1,"PI3",1,"7ML56100BD10"]
["7ML5610-0BD20","Pointek CLS100 RF Capacitance point level switch, PPS process connection. Detects level and interface in liquids, solids, slurries, and foam. Compact, with 100 mm (4 inch) insertion, adaptable sensitivity, with the ability to tune out build-up on probe. . Process connection: R 1\" ((BSPT), EN 10226/PT (JIS-T), JIS B 0203) (PPS probe body) Approvals: General Purpose (CSA, FM) Versions/Options: Enclosure version, PPS process connection, M20x1.5 Overfill Protection: Not Required ",286,"ΤΕΜ",1,"PI3",1,"7ML56100BD20"]
["7ML5631-1AA00-0JB0","Pointek CLS200 RF Capacitance point level switch, cable design. Detects level and interface in liquids, solids, slurries, and foam. Cable extension options to 30 m (98.43 ft), adaptable sensitivity, with the ability to tune out build-up on probe. Process Connection Threaded, 316L (1.4404) stainless steel: R 3/4\" ((BSPT), EN 10226/PT (JIS-T), JIS B 0203) Probe length: (length from flange face) (Threaded lengths include process thread) Extended cable, 3000 mm (118.11\"), length can be shortened by customer Thermal Isolator: Without thermal isolator Wetted Seals: FKM and PTFE Probe Material: FEP Jacketed cable with PPS Probe Body Approvals: General Purpose (CE, C-TICK) Enclosure and Lid: Aluminum epoxy coated 2 x M20 x 1.5 cable inlet, IP65 . ",872,"ΤΕΜ",1,"PI3",1,"7ML56311AA000JB0"]
["7ML5631-1AB00-0JB0","Pointek CLS200 RF Capacitance point level switch, cable design. Detects level and interface in liquids, solids, slurries, and foam. Cable extension options to 30 m (98.43 ft), adaptable sensitivity, with the ability to tune out build-up on probe. Process Connection Threaded, 316L (1.4404) stainless steel: R 3/4\" ((BSPT), EN 10226/PT (JIS-T), JIS B 0203) Probe length: (length from flange face) (threaded lengths include process thread) Extended cable, 6000 mm (236.22\"), length can be shortened by customer Thermal Isolator: Without thermal isolator Wetted Seals: FKM and PTFE Probe Material: FEP Jacketed cable with PPS Probe Body Approvals: General Purpose (CE, C-TICK) Enclosure and Lid: Aluminum epoxy coated 2 x M20 x 1.5 cable inlet, IP65 . ",936,"ΤΕΜ",1,"PI3",1,"7ML56311AB000JB0"]
["7ML5745-1AA02-1AA0","SITRANS LVL100 Vibrating point level switch. Detects level and material in liquids and slurries. Compact, with 40 mm (1.6 inch) insertion. Approvals: ordinary location, CE Process temperature: Standard -40 to 100 C Process connection: Thread G 3/4\" A PN64 / 316L Electronics: Transistor output PNP 10...55 V DC Housing: 316L Electrical connection / Protection: M12x1 / IP67 1 . . ",283,"ΤΕΜ",1,"PI1",1,"7ML57451AA021AA0"]
["7ML5745-1AA42-1AA0","SITRANS LVL100 Vibrating point level switch. Detects level and material in liquids and slurries. Compact, with 40 mm (1.6 inch) insertion. Approvals: ordinary location, CE Process temperature: Standard -40 to 100 C Process connection: Thread G1\" A PN64 / 316L Electronics: Transistor output PNP 10...55 V DC Housing: 316L Electrical connection / Protection: M12x1 / IP67 1 . . ",308,"ΤΕΜ",1,"PI1",1,"7ML57451AA421AA0"]
["7ML5745-1AA02-1BA0","SITRANS LVL100 Vibrating point level switch. Detects level and material in liquids and slurries. Compact, with 40 mm (1.6 inch) insertion. Approvals: ordinary location, CE Process temperature: Standard -40 to 100 C Process connection: Thread G 3/4\" A PN64 / 316L Electronics: Transistor output PNP 10...55 V DC Housing: 316L Electrical connection / Protection: According to ISO4400 including plug / IP65 . . ",298,"ΤΕΜ",1,"PI1",1,"7ML57451AA021BA0"]
["7ML5745-1AA42-1BA0","SITRANS LVL100 Vibrating point level switch. Detects level and material in liquids and slurries. Compact, with 40 mm (1.6 inch) insertion. Approvals: ordinary location, CE Process temperature: Standard -40 to 100 C Process connection: Thread G1\" A PN64 / 316L Electronics: Transistor output PNP 10...55 V DC Housing: 316L Electrical connection / Protection: According to ISO4400 including plug / IP65 . . ",323,"ΤΕΜ",1,"PI1",1,"7ML57451AA421BA0"]
["7ML5735-2AA11-0AA0","SITRANS LVS100 Vibrating fork point level switch: level and material detection for dry bulk solids. Extension options to 4 m (13.12 ft). Input Voltage: DPDT Relay - 19 to 230 V AC, 19 to 40 V DC, (stocked version) Process Temperature: up to +150 C (+302 F) Process connection Threaded: R 1 1/2\" ((BSPT), EN 10226) Extension length: Stainless steel 316L (1.4404): Standard length, 170 mm (6.69 inch) . Approvals: CSA/FM General Purpose, CE, RCM . . ",418,"ΤΕΜ",1,"PI1",1,"7ML57352AA110AA0"]
["7ML5735-1AA11-0BA0","SITRANS LVS100 Vibrating fork point level switch: level and material detection for dry bulk solids. Extension options to 4 m (13.12 ft). Input Voltage: DPDT Relay - 19 to 230 V AC, 19 to 40 V DC Process Temperature: up to +150 C (+302 F) Process connection Threaded: R 1 1/2\" ((BSPT), EN 10226) Extension length: Stainless steel 316L (1.4404): Standard length, 170 mm (6.69 inch) . Approvals: CSA/FM Class II, Div. 1, Group E,F, G, Class III, ATEX II 1/2 D, RCM . . ",608,"ΤΕΜ",1,"PI1",1,"7ML57351AA110BA0"]
["7ML5736-1AA11-1AA0","SITRANS LVS300 Vibrating rod point level switch, compact design: level and material detection in solids. Compact, with 160 mm (6.30 inch) insertion. Power supply: Relays DPDT 21..230V AC 22..45V DC Process temperature: Without temperature isolator (up to Tprocess = 150°C (302°F) at Tamb < 40°C (104°F)) Process connection Threaded: Thread G 1 1/2\" (BSPP) EN ISO 228-1 Extension length: Standard length, 160 mm (6.3 inch) Material process connection/extension: Stainless steel threads 304 (1.4301), tri-clamp 304 (1.4301) Approvals: CE . . ",792,"ΤΕΜ",1,"PI1",1,"7ML57361AA111AA0"]
["7ML5736-1AA11-1BA0","SITRANS LVS300 Vibrating rod point level switch, compact design: level and material detection in solids. Compact, with 160 mm (6.30 inch) insertion. Power supply: Relays DPDT 21..230V AC 22..45V DC Process temperature: Without temperature isolator (up to Tprocess = 150°C (302°F) at Tamb < 40°C (104°F)) Process connection Threaded: Thread G 1 1/2\" (BSPP) EN ISO 228-1 Extension length: Standard length, 160 mm (6.3 inch) Material process connection/extension: Stainless steel threads 304 (1.4301), tri-clamp 304 (1.4301) Approvals: ATEX II 1/2D Ex ta/tb IIIC T! Da/Db IP6X . . ",898,"ΤΕΜ",1,"PI1",1,"7ML57361AA111BA0"]
["7ML5725-5AC11-2AD0","SITRANS LPS200 Rotary paddle point level switch, compact design: level detection in solids. Compact, side or top mount with extension options to 300 mm (11.81 inch). Process temperature: Up to +80 C (+176 F) basic version Aluminum Power supply: 230 V AC, 1 rev/min. Process connection Threaded: G 1-1/2\" ((BSPP), EN ISO 228-1) Process pressure: Up to 0.5 bar (7.25 psi) Process connection material: Aluminum Extension length: 150 mm (5.91 inch) Measuring vane: Boot shaped, 35 x 106 mm (1.38 x 4.17 inch) Approvals: CE, RCM . ",378,"ΤΕΜ",1,"PI1",1,"7ML57255AC112AD0"]
["7ML5725-6ZC12-2AB0 J2A"," SITRANS LPS200 Rotary paddle point level switch, compact design: level detection in solids. Compact, side or top mount with extension options to 300 mm (11.81 inch). Power supply: Universal Voltage, 1 rev/min. Process temperature: Up to +80 C (+176 F) basic version Stainless steel Process connection Threaded: G 1-1/2\" ((BSPP), EN ISO 228-1) Process pressure: Up to 0.5 bar (7.25 psi) Process connection material: Stainless steel 303 (1.4305) flanges 321 (1.4541), tri-clamp 304 (1.4301) Extension length: 150 mm (5.91 inch) Measuring vane: Boot shaped, 35 x 106 mm (1.38 x 4.17 inch) Approvals: ATEX II 1/2 D, RCM .",560,"ΤΕΜ",1,"PI1",1,"7ML57256ZC122AB0J2A"]
["7ML5726-5ZB12-2BA2 J2A"," SITRANS LPS200 Rotary paddle point level switch, shaft protected design: level detection in aggressive solids. Compact, side or top mount, with enhanced shaft protection. Extension options to 300 mm (11.81 inch). Power supply: Universal Voltage, 1 rev/min. Process temperature: Up to +80 C (+176 F) basic version Process connection Threaded: G 1-1/2\" ((BSPP), EN ISO 228-1) Process pressure: Up to 0.5 bar (7.25 psi) Process connection material: Stainless steel threads 303 (1.4305), flanges 321 (1.4541), tri-clamp 304 (1.4301) Extension length: 200 mm (7.87 inch) Extension material (protection tube): Stainless steel 303 (1.4305) Measuring vane: Boot shaped, 35 x 106 mm (1.38 x 4.17 inch) Approvals: ATEX II 1/2 D, RCM",604,"ΤΕΜ",1,"PI1",1,"7ML57265ZB122BA2J2A"]
["7ML5727-5ZB12-0AB0 J2A"," SITRANS LPS200 Rotary paddle point level switch, cable extension design: level detection in solids. Top mount, with extension options to 10 m (32.80 ft). Power supply: Universal Voltage, 1 rev/min. Process temperature: Up to +80 C (+176 F) basic version Process connection Threaded: G 1-1/2\" ((BSPP), EN ISO 228-1) Process pressure: Up to 0.5 bar (7.25 psi) Process connection material: Stainless steel, threads 303 (1.4305),flanges 321 (1.4541) Cable extension length: Standard cable length, 2000 mm (78.74 inch) Measuring vane: Boot shaped, 35 x 106 mm (1.38 x 4.17 inch) Approvals: ATEX II 1/2 D, RCM .",703,"ΤΕΜ",1,"PI1",1,"7ML57275ZB120AB0J2A"]
["7ML1510-1KF01","Pointek ULS200 Ultrasonic point level switch: non-contact, 5 m (16.4 ft) range, for bulk solids, liquids, and slurries. Power supply: 24 VDC, Relay output Approvals: CE, C-TICK, CSA US/C, FM Transducer/Process connection: PVDF copolymer, R 2\" ((BSPT), EN 10226) . Enclosure/cable inlet: Polycarbonate housing, Cable inlet PG 13.5 ",1060,"ΤΕΜ",1,"PI2",1,"7ML15101KF01"]
["7ML1510-1JF02","Pointek ULS200 Ultrasonic point level switch: non-contact, 5 m (16.4 ft) range, for bulk solids, liquids, and slurries. Power supply: 24 VDC, Relay output Approvals: CE, C-TICK CSA Class 1 Div 2, Zone 2, Class II Div 2 Transducer/Process connection: PVDF copolymer, R 2\" ((BSPT), EN 10226) . Enclosure/cable inlet: Polycarbonate housing, Cable inlet 1/2\" NPT ",1060,"ΤΕΜ",1,"PI2",1,"7ML15101JF02"]
["7ML1510-1KB01","Pointek ULS200 Ultrasonic point level switch: non-contact, 5 m (16.4 ft) range, for bulk solids, liquids, and slurries. Power supply: 24 VDC, Relay output Approvals: CE, C-TICK, CSA US/C, FM Transducer/Process connection: EFTE, R 2\" ((BSPT), EN 10226) . Enclosure/cable inlet: Polycarbonate housing, Cable inlet PG 13.5 ",1112,"ΤΕΜ",1,"PI2",1,"7ML15101KB01"]
["7ML1510-1JB02","Pointek ULS200 Ultrasonic point level switch: non-contact, 5 m (16.4 ft) range, for bulk solids, liquids, and slurries. Power supply: 24 VDC, Relay output Approvals: CE, C-TICK CSA Class 1 Div 2, Zone 2, Class II Div 2 Transducer/Process connection: EFTE, R 2\" ((BSPT), EN 10226) . Enclosure/cable inlet: Polycarbonate housing, Cable inlet 1/2\" NPT ",1112,"ΤΕΜ",1,"PI2",1,"7ML15101JB02"]
["7ML1510-3KF01","Pointek ULS200 Ultrasonic point level switch: non-contact, 5 m (16.4 ft) range, for bulk solids, liquids, and slurries. Power supply: 100 to 230 VAC, relay output Approvals: CE, C-TICK, CSA US/C, FM Transducer/Process connection: PVDF copolymer, R 2\" ((BSPT), EN 10226) . Enclosure/cable inlet: Polycarbonate housing, Cable inlet PG 13.5 ",1206,"ΤΕΜ",1,"PI2",1,"7ML15103KF01"]
["7ML1510-3JF02","Pointek ULS200 Ultrasonic point level switch: non-contact, 5 m (16.4 ft) range, for bulk solids, liquids, and slurries. Power supply: 100 to 230 VAC, relay output Approvals: CE, C-TICK CSA Class 1 Div 2, Zone 2, Class II Div 2 Transducer/Process connection: PVDF copolymer, R 2\" ((BSPT), EN 10226) . Enclosure/cable inlet: Polycarbonate housing, Cable inlet 1/2\" NPT ",1206,"ΤΕΜ",1,"PI2",1,"7ML15103JF02"]
["7ML1510-3KB01","Pointek ULS200 Ultrasonic point level switch: non-contact, 5 m (16.4 ft) range, for bulk solids, liquids, and slurries. Power supply: 100 to 230 VAC, relay output Approvals: CE, C-TICK, CSA US/C, FM Transducer/Process connection: EFTE, R 2\" ((BSPT), EN 10226) . Enclosure/cable inlet: Polycarbonate housing, Cable inlet PG 13.5 ",1258,"ΤΕΜ",1,"PI2",1,"7ML15103KB01"]
["7ML1510-3JB02","Pointek ULS200 Ultrasonic point level switch: non-contact, 5 m (16.4 ft) range, for bulk solids, liquids, and slurries. Power supply: 100 to 230 VAC, relay output Approvals: CE, C-TICK CSA Class 1 Div 2, Zone 2, Class II Div 2 Transducer/Process connection: EFTE, R 2\" ((BSPT), EN 10226) . Enclosure/cable inlet: Polycarbonate housing, Cable inlet 1/2\" NPT ",1258,"ΤΕΜ",1,"PI2",1,"7ML15103JB02"]
["7ML5201-0EB0","SITRANS LU150 Ultrasonic level transmitter: continuous, non-contact, 5 m (16.4 ft) range. Monitors level in liquids and slurries. Basic level performance. . Transducer/Process connection: (PVDF)PVDF copolymer, 2\" NPT ((Taper), ANSI/ASME B1.20.1) M20 x 1.5 (General Pupose Cable Gland (-20 to +60 Cel) included) . ",752,"ΤΕΜ",1,"PI2",1,"7ML52010EB0"]
["7ML5201-0FB0","SITRANS LU150 Ultrasonic level transmitter: continuous, non-contact, 5 m (16.4 ft) range. Monitors level in liquids and slurries. Basic level performance. . Transducer/Process connection: PVDF copolymer, R 2\" (BSPT), EN 10226 M20 x 1.5 (General Pupose Cable Gland (-20 to +60 Cel) included) . ",752,"ΤΕΜ",1,"PI2",1,"7ML52010FB0"]
["7ML5201-0GB0","SITRANS LU150 Ultrasonic level transmitter: continuous, non-contact, 5 m (16.4 ft) range. Monitors level in liquids and slurries. Basic level performance. . Transducer/Process connection: PVDF copolymer, G 2\" (BSPP), EN ISO 228-1 M20 x 1.5 (General Pupose Cable Gland (-20 to +60 Cel) included) . ",752,"ΤΕΜ",1,"PI2",1,"7ML52010GB0"]
["7ML5201-0JB0","SITRANS LU150 Ultrasonic level transmitter: continuous, non-contact, 5 m (16.4 ft) range. Monitors level in liquids and slurries. Basic level performance. . Transducer/Process connection: PVDF copolymer, 4\" Sanitary mounting M20 x 1.5 (General Pupose Cable Gland (-20 to +60 Cel) included) . ",832,"ΤΕΜ",1,"PI2",1,"7ML52010JB0"]
["7ML5202-0EB0","SITRANS LU180 Ultrasonic level transmitter: continuous, non-contact, 5 m (16.4 ft) range. Monitors level in liquids and slurries. Basic level performance for intrinsically safe applications. . Transducer/Process connection: PVDF copolymer, 2\" NPT ((Taper), ANSI/ASME B1.20.1) Cable inlet: M20 x 1.5 (General Pupose Cable Gland (-20 to +60 C) included - ",1125,"ΤΕΜ",1,"PI2",1,"7ML52020EB0"]
["7ML5202-0FB0","SITRANS LU180 Ultrasonic level transmitter: continuous, non-contact, 5 m (16.4 ft) range. Monitors level in liquids and slurries. Basic level performance for intrinsically safe applications. . Transducer/Process connection: PVDF copolymer, R 2\" (BSPT), EN 10226 Cable inlet: M20 x 1.5 (General Pupose Cable Gland (-20 to +60 C) included - ",1125,"ΤΕΜ",1,"PI2",1,"7ML52020FB0"]
["7ML5202-0GB0","SITRANS LU180 Ultrasonic level transmitter: continuous, non-contact, 5 m (16.4 ft) range. Monitors level in liquids and slurries. Basic level performance for intrinsically safe applications. . Transducer/Process connection: PVDF copolymer, G 2\" (BSPP), EN ISO 228-1 Cable inlet: M20 x 1.5 (General Pupose Cable Gland (-20 to +60 C) included - ",1125,"ΤΕΜ",1,"PI2",1,"7ML52020GB0"]
["7ML5202-0JB0"," SITRANS LU180 Ultrasonic level transmitter: continuous, non-contact, 5 m (16.4 ft) range. Monitors level in liquids and slurries. Basic level performance for intrinsically safe applications. . Transducer/Process connection: PVDF copolymer, 4\" Sanitary mounting Cable inlet: M20 x 1.5 (General Pupose Cable Gland (-20 to +60 C) included -",1205,"ΤΕΜ",1,"PI2",1,"7ML52020JB0"]
["7ML1830-1DT","LOCKNUT, 2\" NPT, Nylon",18,"ΤΕΜ",1,"PI2",1,"7ML18301DT"]
["7ML1830-1DQ","LOCKNUT,2\" BSPT, PLASTIC",18,"ΤΕΜ",1,"PI2",1,"7ML18301DQ"]
["7ML1830-1BR","Sanitary 4 inch mounting clamp",78,"ΤΕΜ",1,"PI2",1,"7ML18301BR"]
["7ML5110-1EE07-4AF3","SITRANS Probe LU240 Ultrasonic level transmitter ideal for level, volume, and volume flow measurements. It works with liquids, slurries, and bulk materials up to 12 m (40 ft). Process connection: R 2\" . Process connection: R 2\" [(BSPT), EN 10226] . Type of protection: Non Ex (ordinary locations) cCSAus, Local HMI: With display (clear lid of PC material) ",1252,"ΤΕΜ",1,"PI2",1,"7ML51101EE074AF3"]
["7ML5110-1DE07-4AF3  ","SITRANS Probe LU240 Ultrasonic level transmitter ideal for level, volume, and volume flow measurements. It works with liquids, slurries, and bulk materials up to 12 m (40 ft). . Communications: HART (4 ... 20 mA) level, volume, volume flow Ingress protection: IP66, IP68, TYPE 4X, 6 Measurement range/ wetted parts: 200 ... 6000 mm (7.87 ... 236.22 inch), PVDF Copolymer Process connection: R 2\" [(BSPT), EN 10226] . Non wetted parts: Plastic (PBT/PC material) Enclosure Type of protection: Non Ex (ordinary locations) cCSAus, CE, RCM, EAC Electrical connections/ cable entries: 2 x M20 x 1.5 (one general purpose Polyamide cable gland and one Polyamide blocking plug provided) Local HMI: With display (clear lid of PC material) ",1178,"ΤΕΜ",1,"PI2",1,"7ML51101DE074AF3"]
["7ML5110-1HE07-4AF3  ","SITRANS Probe LU240 Ultrasonic level transmitter ideal for level, volume, and volume flow measurements. It works with liquids, slurries, and bulk materials up to 12 m (40 ft). Process connection: R 2\" . Process connection: R 2\" [(BSPT), EN 10226] . Type of protection: Non Ex (ordinary locations) cCSAus, Local HMI: With display (clear lid of PC material) ",1349,"ΤΕΜ",1,"PI2",1,"7ML51101HE074AF3"]
["7ML5110-1GE07-4AF3  ","SITRANS Probe LU240 Ultrasonic level transmitter ideal for level, volume, and volume flow measurements. It works with liquids, slurries, and bulk materials up to 12 m (40 ft). . Communications: HART (4 ... 20 mA) level, volume, volume flow Ingress protection: IP66, IP68, TYPE 4X, 6 Measurement range/ wetted parts: 200 ... 12000 mm (7.87 ... 472.44 inch), PVDF Copolymer Process connection: R 2\" [(BSPT), EN 10226] . Non wetted parts: Plastic (PBT/PC material) Enclosure Type of protection: Non Ex (ordinary locations) cCSAus, CE, RCM, EAC Electrical connections/ cable entries: 2 x M20 x 1.5 (one general purpose Polyamide cable gland and one Polyamide blocking plug provided) Local HMI: With display (clear lid of PC material) ",1276,"ΤΕΜ",1,"PI2",1,"7ML51101GE074AF3"]
["7ML5050-0AC12-1DA0","SITRANS LUT400 Series Ultrasonic level controller: continuous, non-contact, 60 m (197 ft) range. Monitors level, volume, and volume flow in liquids, slurries, and solids. With high accuracy volume flow and built in data logging. - Model: SITRANS LUT420 - Level controller Enclosure Display Options: No display (blank lid provided) Input Voltage: 100 to 230 V AC +/- 15% Cable Inlet: 3 cable inlets, 3 M20 plastic cable glands supplied Number of measurement points: Single point system (includes one transducer input,one mA output and one external temperature sensor input) Communications & I/O: HART, 2 discrete inputs, 3 relays Approvals: General Purpose CE, FM, CSA US/C, UL, RCM,EAC,KCC - ",1068,"ΤΕΜ",1,"PI2",1,"7ML5050-0AC12-1DA0"]
["7ML5050-0AC12-1DC0"," SITRANS LUT400 Series Ultrasonic level controller: continuous, non-contact, 60 m (197 ft) range. Monitors level, volume, and volume flow in liquids, slurries, and solids. With high accuracy volume flow and built in data logging. - Model: SITRANS LUT420 - Level controller Enclosure Display Options: No display (blank lid provided) Input Voltage: 100 to 230 V AC +/- 15% Cable Inlet: 3 cable inlets, 3 M20 plastic cable glands supplied Number of measurement points: Single point system (includes one transducer input,one mA output and one external temperature sensor input) Communications & I/O: HART, 2 discrete inputs, 3 relays Approvals: Hazardous locations CSA Class I, II, III Division 2 (Groups A,B,C,D,F,G) -",1142,"ΤΕΜ",1,"PI2",1,"7ML50500AC121DC0"]
["7ML5050-0AC22-1DA0","SITRANS LUT400 Series Ultrasonic level controller: continuous, non-contact, 60 m (197 ft) range. Monitors level, volume, and volume flow in liquids, slurries, and solids. With high accuracy volume flow and built in data logging. - Model: SITRANS LUT420 - Level controller Enclosure Display Options: No display (blank lid provided) Input Voltage: 10 to 32 V DC Cable Inlet: 3 cable inlets, 3 M20 plastic cable glands supplied Number of measurement points: Single point system (includes one transducer input,one mA output and one external temperature sensor input) Communications & I/O: HART, 2 discrete inputs, 3 relays Approvals: General Purpose CE, FM, CSA US/C, UL, RCM,EAC,KCC - ",1068,"ΤΕΜ",1,"PI2",1,"7ML50500AC221DA0"]
["7ML5050-0AC22-1DC0"," SITRANS LUT400 Series Ultrasonic level controller: continuous, non-contact, 60 m (197 ft) range. Monitors level, volume, and volume flow in liquids, slurries, and solids. With high accuracy volume flow and built in data logging. - Model: SITRANS LUT420 - Level controller Enclosure Display Options: No display (blank lid provided) Input Voltage: 10 to 32 V DC Cable Inlet: 3 cable inlets, 3 M20 plastic cable glands supplied Number of measurement points: Single point system (includes one transducer input,one mA output and one external temperature sensor input) Communications & I/O: HART, 2 discrete inputs, 3 relays Approvals: Hazardous locations CSA Class I, II, III Division 2 (Groups A,B,C,D,F,G) -",1142,"ΤΕΜ",1,"PI2",1,"7ML50500AC221DC0"]
["7ML5050-0AA12-1DA0","SITRANS LUT400 Series Ultrasonic level controller: continuous, non-contact, 60 m (197 ft) range. Monitors level, volume, and volume flow in liquids, slurries, and solids. With high accuracy volume flow and built in data logging. - Model: SITRANS LUT420 - Level controller Enclosure Display Options: With display Input Voltage: 100 to 230 V AC +/- 15% Cable Inlet: 3 cable inlets, 3 M20 plastic cable glands supplied Number of measurement points: Single point system (includes one transducer input,one mA output and one external temperature sensor input) Communications & I/O: HART, 2 discrete inputs, 3 relays Approvals: General Purpose CE, FM, CSA US/C, UL, RCM,EAC,KCC - ",1220,"ΤΕΜ",1,"PI2",1,"7ML50500AA121DA0"]
["7ML5050-0AA12-1DC0","SITRANS LUT400 Series Ultrasonic level controller: continuous, non-contact, 60 m (197 ft) range. Monitors level, volume, and volume flow in liquids, slurries, and solids. With high accuracy volume flow and built in data logging. - Model: SITRANS LUT420 - Level controller Enclosure Display Options: With display Input Voltage: 100 to 230 V AC +/- 15% Cable Inlet: 3 cable inlets, 3 M20 plastic cable glands supplied Number of measurement points: Single point system (includes one transducer input,one mA output and one external temperature sensor input) Communications & I/O: HART, 2 discrete inputs, 3 relays Approvals: Hazardous locations CSA Class I, II, III Division 2 (Groups A,B,C,D,F,G) - ",1295,"ΤΕΜ",1,"PI2",1,"7ML50500AA121DC0"]
["7ML5050-0AA22-1DA0","SITRANS LUT400 Series Ultrasonic level controller: continuous, non-contact, 60 m (197 ft) range. Monitors level, volume, and volume flow in liquids, slurries, and solids. With high accuracy volume flow and built in data logging. - Model: SITRANS LUT420 - Level controller Enclosure Display Options: With display Input Voltage: 10 to 32 V DC Cable Inlet: 3 cable inlets, 3 M20 plastic cable glands supplied Number of measurement points: Single point system (includes one transducer input,one mA output and one external temperature sensor input) Communications & I/O: HART, 2 discrete inputs, 3 relays Approvals: General Purpose CE, FM, CSA US/C, UL, RCM,EAC,KCC - ",1220,"ΤΕΜ",1,"PI2",1,"7ML50500AA221DA0"]
["7ML5050-0AA22-1DC0","SITRANS LUT400 Series Ultrasonic level controller: continuous, non-contact, 60 m (197 ft) range. Monitors level, volume, and volume flow in liquids, slurries, and solids. With high accuracy volume flow and built in data logging. - Model: SITRANS LUT420 - Level controller Enclosure Display Options: With display Input Voltage: 10 to 32 V DC Cable Inlet: 3 cable inlets, 3 M20 plastic cable glands supplied Number of measurement points: Single point system (includes one transducer input,one mA output and one external temperature sensor input) Communications & I/O: HART, 2 discrete inputs, 3 relays Approvals: Hazardous locations CSA Class I, II, III Division 2 (Groups A,B,C,D,F,G) - ",1295,"ΤΕΜ",1,"PI2",1,"7ML50500AA221DC0"]
["7ML5050-0AB12-1DA0","SITRANS LUT400 Series Ultrasonic level controller: continuous, non-contact, 60 m (197 ft) range. Monitors level, volume, and volume flow in liquids, slurries, and solids. With high accuracy volume flow and built in data logging. - Model: SITRANS LUT420 - Level controller Enclosure Display Options: With remote panel mount display Input Voltage: 100 to 230 V AC +/- 15% Cable Inlet: 3 cable inlets, 3 M20 plastic cable glands supplied Number of measurement points: Single point system (includes one transducer input,one mA output and one external temperature sensor input) Communications & I/O: HART, 2 discrete inputs, 3 relays Approvals: General Purpose CE, FM, CSA US/C, UL, RCM,EAC,KCC - ",1412,"ΤΕΜ",1,"PI2",1,"7ML50500AB121DA0"]
["7ML5050-0AB12-1DC0","SITRANS LUT400 Series Ultrasonic level controller: continuous, non-contact, 60 m (197 ft) range. Monitors level, volume, and volume flow in liquids, slurries, and solids. With high accuracy volume flow and built in data logging. - Model: SITRANS LUT420 - Level controller Enclosure Display Options: With remote panel mount display Input Voltage: 100 to 230 V AC +/- 15% Cable Inlet: 3 cable inlets, 3 M20 plastic cable glands supplied Number of measurement points: Single point system (includes one transducer input,one mA output and one external temperature sensor input) Communications & I/O: HART, 2 discrete inputs, 3 relays Approvals: Hazardous locations CSA Class I, II, III Division 2 (Groups A,B,C,D,F,G) - ",1487,"ΤΕΜ",1,"PI2",1,"7ML50500AB121DC0"]
["7ML5050-0AB22-1DA0","SITRANS LUT400 Series Ultrasonic level controller: continuous, non-contact, 60 m (197 ft) range. Monitors level, volume, and volume flow in liquids, slurries, and solids. With high accuracy volume flow and built in data logging. - Model: SITRANS LUT420 - Level controller Enclosure Display Options: With remote panel mount display Input Voltage: 10 to 32 V DC Cable Inlet: 3 cable inlets, 3 M20 plastic cable glands supplied Number of measurement points: Single point system (includes one transducer input,one mA output and one external temperature sensor input) Communications & I/O: HART, 2 discrete inputs, 3 relays Approvals: General Purpose CE, FM, CSA US/C, UL, RCM,EAC,KCC - ",1412,"ΤΕΜ",1,"PI2",1,"7ML50500AB221DA0"]
["7ML5050-0AB22-1DC0","SITRANS LUT400 Series Ultrasonic level controller: continuous, non-contact, 60 m (197 ft) range. Monitors level, volume, and volume flow in liquids, slurries, and solids. With high accuracy volume flow and built in data logging. - Model: SITRANS LUT420 - Level controller Enclosure Display Options: With remote panel mount display Input Voltage: 10 to 32 V DC Cable Inlet: 3 cable inlets, 3 M20 plastic cable glands supplied Number of measurement points: Single point system (includes one transducer input,one mA output and one external temperature sensor input) Communications & I/O: HART, 2 discrete inputs, 3 relays Approvals: Hazardous locations CSA Class I, II, III Division 2 (Groups A,B,C,D,F,G) - ",1487,"ΤΕΜ",1,"PI2",1,"7ML50500AB221DC0"]
["7ML5050-0BC12-1DA0","SITRANS LUT400 Series Ultrasonic level controller: continuous, non-contact, 60 m (197 ft) range. Monitors level, volume, and volume flow in liquids, slurries, and solids. With high accuracy volume flow and built in data logging. - Model: SITRANS LUT430 - Level, Pump & Flow controller Enclosure Display Options: No display (blank lid provided) Input Voltage: 100 to 230 V AC +/- 15% Cable Inlet: 3 cable inlets, 3 M20 plastic cable glands supplied Number of measurement points: Single point system (includes one transducer input,one mA output and one external temperature sensor input) Communications & I/O: HART, 2 discrete inputs, 3 relays Approvals: General Purpose CE, FM, CSA US/C, UL, RCM,EAC,KCC - ",1540,"ΤΕΜ",1,"PI2",1,"7ML50500BC121DA0"]
["7ML5050-0BC12-1DC0"," SITRANS LUT400 Series Ultrasonic level controller: continuous, non-contact, 60 m (197 ft) range. Monitors level, volume, and volume flow in liquids, slurries, and solids. With high accuracy volume flow and built in data logging. - Model: SITRANS LUT430 - Level, Pump & Flow controller Enclosure Display Options: No display (blank lid provided) Input Voltage: 100 to 230 V AC +/- 15% Cable Inlet: 3 cable inlets, 3 M20 plastic cable glands supplied Number of measurement points: Single point system (includes one transducer input,one mA output and one external temperature sensor input) Communications & I/O: HART, 2 discrete inputs, 3 relays Approvals: Hazardous locations CSA Class I, II, III Division 2 (Groups A,B,C,D,F,G) -",1615,"ΤΕΜ",1,"PI2",1,"7ML50500BC121DC0"]
["7ML5050-0BC22-1DA0"," SITRANS LUT400 Series Ultrasonic level controller: continuous, non-contact, 60 m (197 ft) range. Monitors level, volume, and volume flow in liquids, slurries, and solids. With high accuracy volume flow and built in data logging. - Model: SITRANS LUT430 - Level, Pump & Flow controller Enclosure Display Options: No display (blank lid provided) Input Voltage: 10 to 32 V DC Cable Inlet: 3 cable inlets, 3 M20 plastic cable glands supplied Number of measurement points: Single point system (includes one transducer input,one mA output and one external temperature sensor input) Communications & I/O: HART, 2 discrete inputs, 3 relays Approvals: General Purpose CE, FM, CSA US/C, UL, RCM,EAC,KCC -",1540,"ΤΕΜ",1,"PI2",1,"7ML50500BC221DA0"]
["7ML5050-0BC22-1DC0"," SITRANS LUT400 Series Ultrasonic level controller: continuous, non-contact, 60 m (197 ft) range. Monitors level, volume, and volume flow in liquids, slurries, and solids. With high accuracy volume flow and built in data logging. - Model: SITRANS LUT430 - Level, Pump & Flow controller Enclosure Display Options: No display (blank lid provided) Input Voltage: 10 to 32 V DC Cable Inlet: 3 cable inlets, 3 M20 plastic cable glands supplied Number of measurement points: Single point system (includes one transducer input,one mA output and one external temperature sensor input) Communications & I/O: HART, 2 discrete inputs, 3 relays Approvals: Hazardous locations CSA Class I, II, III Division 2 (Groups A,B,C,D,F,G) -",1615,"ΤΕΜ",1,"PI2",1,"7ML50500BC221DC0"]
["7ML5050-0BA12-1DA0","SITRANS LUT400 Series Ultrasonic level controller: continuous, non-contact, 60 m (197 ft) range. Monitors level, volume, and volume flow in liquids, slurries, and solids. With high accuracy volume flow and built in data logging. - Model: SITRANS LUT430 - Level, Pump & Flow controller Enclosure Display Options: With display Input Voltage: 100 to 230 V AC +/- 15% Cable Inlet: 3 cable inlets, 3 M20 plastic cable glands supplied Number of measurement points: Single point system (includes one transducer input,one mA output and one external temperature sensor input) Communications & I/O: HART, 2 discrete inputs, 3 relays Approvals: General Purpose CE, FM, CSA US/C, UL, RCM,EAC,KCC - ",1693,"ΤΕΜ",1,"PI2",1,"7ML50500BA121DA0"]
["7ML5050-0BA12-1DC0","SITRANS LUT400 Series Ultrasonic level controller: continuous, non-contact, 60 m (197 ft) range. Monitors level, volume, and volume flow in liquids, slurries, and solids. With high accuracy volume flow and built in data logging. - Model: SITRANS LUT430 - Level, Pump & Flow controller Enclosure Display Options: With display Input Voltage: 100 to 230 V AC +/- 15% Cable Inlet: 3 cable inlets, 3 M20 plastic cable glands supplied Number of measurement points: Single point system (includes one transducer input,one mA output and one external temperature sensor input) Communications & I/O: HART, 2 discrete inputs, 3 relays Approvals: Hazardous locations CSA Class I, II, III Division 2 (Groups A,B,C,D,F,G) - ",1767,"ΤΕΜ",1,"PI2",1,"7ML50500BA121DC0"]
["7ML5050-0BA22-1DA0","SITRANS LUT400 Series Ultrasonic level controller: continuous, non-contact, 60 m (197 ft) range. Monitors level, volume, and volume flow in liquids, slurries, and solids. With high accuracy volume flow and built in data logging. - Model: SITRANS LUT430 - Level, Pump & Flow controller Enclosure Display Options: With display Input Voltage: 10 to 32 V DC Cable Inlet: 3 cable inlets, 3 M20 plastic cable glands supplied Number of measurement points: Single point system (includes one transducer input,one mA output and one external temperature sensor input) Communications & I/O: HART, 2 discrete inputs, 3 relays Approvals: General Purpose CE, FM, CSA US/C, UL, RCM,EAC,KCC - ",1693,"ΤΕΜ",1,"PI2",1,"7ML50500BA221DA0"]
["7ML5050-0BA22-1DC0"," SITRANS LUT400 Series Ultrasonic level controller: continuous, non-contact, 60 m (197 ft) range. Monitors level, volume, and volume flow in liquids, slurries, and solids. With high accuracy volume flow and built in data logging. - Model: SITRANS LUT430 - Level, Pump & Flow controller Enclosure Display Options: With display Input Voltage: 10 to 32 V DC Cable Inlet: 3 cable inlets, 3 M20 plastic cable glands supplied Number of measurement points: Single point system (includes one transducer input,one mA output and one external temperature sensor input) Communications & I/O: HART, 2 discrete inputs, 3 relays Approvals: Hazardous locations CSA Class I, II, III Division 2 (Groups A,B,C,D,F,G) -",1767,"ΤΕΜ",1,"PI2",1,"7ML50500BA221DC0"]
["7ML5050-0BB12-1DA0","SITRANS LUT400 Series Ultrasonic level controller: continuous, non-contact, 60 m (197 ft) range. Monitors level, volume, and volume flow in liquids, slurries, and solids. With high accuracy volume flow and built in data logging. - Model: SITRANS LUT430 - Level, Pump & Flow controller Enclosure Display Options: With remote panel mount display Input Voltage: 100 to 230 V AC +/- 15% Cable Inlet: 3 cable inlets, 3 M20 plastic cable glands supplied Number of measurement points: Single point system (includes one transducer input,one mA output and one external temperature sensor input) Communications & I/O: HART, 2 discrete inputs, 3 relays Approvals: General Purpose CE, FM, CSA US/C, UL, RCM,EAC,KCC - ",1884,"ΤΕΜ",1,"PI2",1,"7ML50500BB121DA0"]
["7ML5050-0BB12-1DC0"," SITRANS LUT400 Series Ultrasonic level controller: continuous, non-contact, 60 m (197 ft) range. Monitors level, volume, and volume flow in liquids, slurries, and solids. With high accuracy volume flow and built in data logging. - Model: SITRANS LUT430 - Level, Pump & Flow controller Enclosure Display Options: With remote panel mount display Input Voltage: 100 to 230 V AC +/- 15% Cable Inlet: 3 cable inlets, 3 M20 plastic cable glands supplied Number of measurement points: Single point system (includes one transducer input,one mA output and one external temperature sensor input) Communications & I/O: HART, 2 discrete inputs, 3 relays Approvals: Hazardous locations CSA Class I, II, III Division 2 (Groups A,B,C,D,F,G) -",1959,"ΤΕΜ",1,"PI2",1,"7ML50500BB121DC0"]
["7ML5050-0BB22-1DA0","SITRANS LUT400 Series Ultrasonic level controller: continuous, non-contact, 60 m (197 ft) range. Monitors level, volume, and volume flow in liquids, slurries, and solids. With high accuracy volume flow and built in data logging. - Model: SITRANS LUT430 - Level, Pump & Flow controller Enclosure Display Options: With remote panel mount display Input Voltage: 10 to 32 V DC Cable Inlet: 3 cable inlets, 3 M20 plastic cable glands supplied Number of measurement points: Single point system (includes one transducer input,one mA output and one external temperature sensor input) Communications & I/O: HART, 2 discrete inputs, 3 relays Approvals: General Purpose CE, FM, CSA US/C, UL, RCM,EAC,KCC - ",1884,"ΤΕΜ",1,"PI2",1,"7ML50500BB221DA0"]
["7ML5050-0BB22-1DC0","SITRANS LUT400 Series Ultrasonic level controller: continuous, non-contact, 60 m (197 ft) range. Monitors level, volume, and volume flow in liquids, slurries, and solids. With high accuracy volume flow and built in data logging. - Model: SITRANS LUT430 - Level, Pump & Flow controller Enclosure Display Options: With remote panel mount display Input Voltage: 10 to 32 V DC Cable Inlet: 3 cable inlets, 3 M20 plastic cable glands supplied Number of measurement points: Single point system (includes one transducer input,one mA output and one external temperature sensor input) Communications & I/O: HART, 2 discrete inputs, 3 relays Approvals: Hazardous locations CSA Class I, II, III Division 2 (Groups A,B,C,D,F,G) - ",1959,"ΤΕΜ",1,"PI2",1,"7ML50500BB221DC0"]
["7ML1930-1GE","KIT, SITRANS LUT400 SUN SHIELD KIT, 304 STAINLESS STEEL ",280,"ΤΕΜ",1,"PI2",1,"7ML19301GE"]
["7ML5034-5AA01","HydroRanger 200 Ultrasonic level controller: continuous, non-contact, 15 m (50 ft) range. Monitors level, volume, and open channel flow in liquids, slurries, and solids. Mounting: 4 button HMI, Wall mount, 4 entries, 4 M20 cable glands included Input voltage: 100 to 230 VAC Number of measurement points: Single point model, 6 relays Data Communications: Without module Approvals: General Purpose CE, FM, CSA US/C , UL listed, RCM, EAC, KCC ",1664,"ΤΕΜ",1,"PI2",1,"7ML50345AA01"]
["7ML5034-5AA02"," HydroRanger 200 Ultrasonic level controller: continuous, non-contact, 15 m (50 ft) range. Monitors level, volume, and open channel flow in liquids, slurries, and solids. Mounting: 4 button HMI, Wall mount, 4 entries, 4 M20 cable glands included Input voltage: 100 to 230 VAC Number of measurement points: Single point model, 6 relays Data Communications: Without module Approvals: CSA Class I, Div.2, Group A,B,C and D; Class II, DIV 2, Group F and G, Class III (for wall mount applications only)",1741,"ΤΕΜ",1,"PI2",1,"7ML50345AA02"]
["7ML5034-5BA01","HydroRanger 200 Ultrasonic level controller: continuous, non-contact, 15 m (50 ft) range. Monitors level, volume, and open channel flow in liquids, slurries, and solids. Mounting: 4 button HMI, Wall mount, 4 entries, 4 M20 cable glands included Input voltage: 12 to 30 VDC Number of measurement points: Single point model, 6 relays Data Communications: Without module Approvals: General Purpose CE, FM, CSA US/C , UL listed, RCM, EAC, KCC ",1664,"ΤΕΜ",1,"PI2",1,"7ML50345BA01"]
["7ML5034-5BA02"," HydroRanger 200 Ultrasonic level controller: continuous, non-contact, 15 m (50 ft) range. Monitors level, volume, and open channel flow in liquids, slurries, and solids. Mounting: 4 button HMI, Wall mount, 4 entries, 4 M20 cable glands included Input voltage: 12 to 30 VDC Number of measurement points: Single point model, 6 relays Data Communications: Without module Approvals: CSA Class I, Div.2, Group A,B,C and D; Class II, DIV 2, Group F and G, Class III (for wall mount applications only)",1741,"ΤΕΜ",1,"PI2",1,"7ML50345BA02"]
["7ML5034-5AB01","HydroRanger 200 Ultrasonic level controller: continuous, non-contact, 15 m (50 ft) range. Monitors level, volume, and open channel flow in liquids, slurries, and solids. Mounting: 4 button HMI, Wall mount, 4 entries, 4 M20 cable glands included Input voltage: 100 to 230 VAC Number of measurement points: Dual point model, 6 relays Data Communications: Without module Approvals: General Purpose CE, FM, CSA US/C , UL listed, RCM, EAC, KCC ",1958,"ΤΕΜ",1,"PI2",1,"7ML50345AB01"]
["7ML5034-5AB02","HydroRanger 200 Ultrasonic level controller: continuous, non-contact, 15 m (50 ft) range. Monitors level, volume, and open channel flow in liquids, slurries, and solids. Mounting: 4 button HMI, Wall mount, 4 entries, 4 M20 cable glands included Input voltage: 100 to 230 VAC Number of measurement points: Dual point model, 6 relays Data Communications: Without module Approvals: CSA Class I, Div.2, Group A,B,C and D; Class II, DIV 2, Group F and G, Class III (for wall mount applications only) ",2035,"ΤΕΜ",1,"PI2",1,"7ML50345AB02"]
["7ML5034-5BB01","HydroRanger 200 Ultrasonic level controller: continuous, non-contact, 15 m (50 ft) range. Monitors level, volume, and open channel flow in liquids, slurries, and solids. Mounting: 4 button HMI, Wall mount, 4 entries, 4 M20 cable glands included Input voltage: 12 to 30 VDC Number of measurement points: Dual point model, 6 relays Data Communications: Without module Approvals: General Purpose CE, FM, CSA US/C , UL listed, RCM, EAC, KCC ",1958,"ΤΕΜ",1,"PI2",1,"7ML50345BB01"]
["7ML5034-5BB02"," HydroRanger 200 Ultrasonic level controller: continuous, non-contact, 15 m (50 ft) range. Monitors level, volume, and open channel flow in liquids, slurries, and solids. Mounting: 4 button HMI, Wall mount, 4 entries, 4 M20 cable glands included Input voltage: 12 to 30 VDC Number of measurement points: Dual point model, 6 relays Data Communications: Without module Approvals: CSA Class I, Div.2, Group A,B,C and D; Class II, DIV 2, Group F and G, Class III (for wall mount applications only)",2035,"ΤΕΜ",1,"PI2",1,"7ML50345BB02"]
["7ML1930-1GA","Sun shield kit, 304 stainless steel",338,"ΤΕΜ",1,"PI2",1,"7ML19301GA"]
["7ML1106-2AA20-0A","EchoMax XRS-5 Ultrasonic level transducer: continuous, non-contact, 8 m (26 ft) range, for liquids and slurries. Mounting thread: R 1\" ((BSPT), EN 10226) Cable length: 5 m (16.40 ft) Facing: Standard (CSM rubber) Approvals: FM Class I Zone 1, ATEX II 2GD, CSA Class I Div. 2, SAA Ex s Class I Zone 1 & DIP Practice A Zone 20 . . Flange: Without mounting flange ",591,"ΤΕΜ",1,"PI2",1,"7ML11062AA200A"]
["7ML1115-3BA30","EchoMax XPS-10 Ultrasonic level transducer: continuous, non-contact, 10 m (32.80 ft), for liquids and solids. Mounting thread and facing: R 1\" ((BSPT) EN 10226-1) Cable length: 5 m (16.40 ft) Flange, flush mount: No flange Approvals: ATEX II 2GD,FM Class I Div 2/SAA Class 1 Zone 1 . ",637,"ΤΕΜ",1,"PI2",1,"7ML11153BA30"]
["7ML1118-3BA30","EchoMax XPS-15 Ultrasonic level transducer: continuous, non-contact, 15 m (49.21 ft), for liquids and solids. Mounting thread and facing: R 1\" ((BSPT) EN 10226-1) Cable length: 5 m (16.40 ft) Flange: No Mounting flange Approvals: ATEX II 2GD, FM Class I Div 2/SAA Class 1 Zone 1 Manual: Multi-Language,Quick Start ",901,"ΤΕΜ",1,"PI2",1,"7ML11183BA30"]
["7ML1100-1AA30","ST-H Ultrasonic level transducer: continuous, non-contact, 0.3 m (1 ft) range, for liquids. Process connection: ETFE, R 2\" ((BSPT), EN 10226) Cable length: 5 m (16.40 ft) . Approvals: ATEX II 2G, CSA C-TICK, INMETRO . ",706,"ΤΕΜ",1,"PI2",1,"7ML11001AA30"]
["7ML1123-0BA50","EchoMax XPS-30 Ultrasonic level transducer: continuous, non-contact, 30 m (98.42 ft) for liquids and solids. Mounting thread and facing: 1 1/2\" universal thread Cable length: 5 m (16.40 ft) Flange: Without mounting flange Approvals: ATEX II 2G 1D, FM Class 1 Div 2, SAA Instruction Manual: Multi-Language Quick Start ",1469,"ΤΕΜ",1,"PI2",1,"7ML11230BA50"]
["7ML1830-1DR","Locknut,1\" bsp,plain",14,"ΤΕΜ",1,"PI2",1,"7ML18301DR"]
["7ML1830-1AN","EASY AIMER II, ALUMINIUM, 3/4 INCH NTP WITH 1 - 11/2 INCH GALVANIZED COUPLING (FOR USE WITH XPS-30 OR XPS-40. TRANSDUCERS ONLY) ",163,"ΤΕΜ",1,"PI2",1,"7ML18301AN"]
["7ML1830-1AP","EASY AIMER II, ALUMINIUM, 3/4 INCH NPT WITH 1 INCH GALVANIZED COUPLING ",163,"ΤΕΜ",1,"PI2",1,"7ML18301AP"]
["7ML1830-1AQ","EASY AIMER II, ALUMINIUM, 3/4 INCH NTP WITH 3/4 - 1 INCH PVC COUPLING ",163,"ΤΕΜ",1,"PI2",1,"7ML18301AQ"]
["7ML1830-1AX","Easy Aimer II Flange, Aluminium with M20 Adapter, 1\" and 1-1/2 \" BSP aluminium coupling. ",230,"ΤΕΜ",1,"PI2",1,"7ML18301AX"]
["7ML1830-1BH","SHIELD,SUBMERGENCE,KIT,for XPS10/XRS-5 sensors ",35,"ΤΕΜ",1,"PI2",1,"7ML18301BH"]
["7ML1830-1BJ","SHIELD,SUBMERGENCE,KIT, for XPS15 sensors ",41,"ΤΕΜ",1,"PI2",1,"7ML18301BJ"]
["7ML1830-1BK","UNIVERSAL BOX BRACKET, FMS-200",158,"ΤΕΜ",1,"PI2",1,"7ML18301BK"]
["7ML1830-1BL","CHANNEL BRACKET,WALL MOUNT, FMS-210 ",229,"ΤΕΜ",1,"PI2",1,"7ML18301BL"]
["7ML1830-1BM","EXTENDED CHANNEL BRACKET, WALL MOUNT FMS-220 ",395,"ΤΕΜ",1,"PI2",1,"7ML18301BM"]
["7ML1830-1BN","CHANNEL BRACKET,FLOOR MOUNT FMS-310 ",378,"ΤΕΜ",1,"PI2",1,"7ML18301BN"]
["7ML1830-1BP","EXTENDED CHANNEL BRACKET,FLOOR MOUNT, FMS-320 ",541,"ΤΕΜ",1,"PI2",1,"7ML18301BP"]
["7ML1830-1BQ","BRIDGE CHANNEL BRACKET, FLOOR MOUNT, FMS-350 ",890,"ΤΕΜ",1,"PI2",1,"7ML18301BQ"]
["7ML5307-1AA06-0AA0","SITRANS LR100 Radar level transmitter, continuous, non-contact, 8 m (26 ft) range, for liquids and slurries, integrated 8 m (26 ft) cable connection. . . . Process connection: 1-1/2\" NPT [(Taper), ASME B1.20.1] / electrical connection 1\"NPT . . . . . . ",617,"ΤΕΜ",1,"PI1",1,"7ML53071AA060AA0"]
["7ML5307-1AB06-0AA0","SITRANS LR100 Radar level transmitter, continuous, non-contact, 8 m (26 ft) range, for liquids and slurries, integrated 8 m (26 ft) cable connection. . . . Process connection: R 1-1/2\" [(BSPT), EN 10226] / electrical connection 1\" BSPT . . . . . . ",617,"ΤΕΜ",1,"PI1",1,"7ML53071AB060AA0"]
["7ML5310-1AA06-0AA0","SITRANS LR110 Radar level transmitter, continuous, non-contact, 15m (49.2ft) range, for liquids, slurries, or solids, integrated cable connection. Communications: HART (4 ... 20 mA) Bluetooth function: Enabled Cable length: 5m Process connection: 1-1/2\" NPT [(Taper), ASME B1.20.1]/ electrical connection 1\" NPT . Type of protection: Non Ex . . ",855,"ΤΕΜ",1,"PI1",1,"7ML53101AA060AA0"]
["7ML5310-1BA06-0AA0  ","SITRANS LR110 Radar level transmitter, continuous, non-contact, 15m (49.2ft) range, for liquids, slurries, or solids, integrated cable connection. Communications: HART (4 ... 20 mA) Bluetooth function: Enabled Cable length: 10m Process connection: 1-1/2\" NPT [(Taper), ASME B1.20.1]/ electrical connection 1\" NPT . . . Type of protection: Non Ex (ordinary locations) cFMus, cCSAus,CE, RCM . . ",872,"ΤΕΜ",1,"PI1",1,"7ML53101BA060AA0"]
["7ML5310-1CA06-0AA0","SITRANS LR110 Radar level transmitter, continuous, non-contact, 15m (49.2ft) range, for liquids, slurries, or solids, integrated cable connection. Communications: HART (4 ... 20 mA) Bluetooth function: Enabled Cable length: 30m Process connection: 1-1/2\" NPT [(Taper), ASME B1.20.1]/ electrical connection 1\" NPT . . . Type of protection: Non Ex (ordinary locations) cFMus, cCSAus,CE, RCM . . ",940,"ΤΕΜ",1,"PI1",1,"7ML53101CA060AA0"]
["7ML5310-1DA06-0AA0  ","SITRANS LR110 Radar level transmitter, continuous, non-contact, 15m (49.2ft) range, for liquids, slurries, or solids, integrated cable connection. Communications: HART (4 ... 20 mA) Bluetooth function: Enabled Cable length: 50m Process connection: 1-1/2\" NPT [(Taper), ASME B1.20.1]/ electrical connection 1\" NPT . Type of protection: Non Ex . . ",1007,"ΤΕΜ",1,"PI1",1,"7ML53101DA060AA0"]
["7ML5310-1EA06-0AA0  ","SITRANS LR110 Radar level transmitter, continuous, non-contact, 15m (49.2ft) range, for liquids, slurries, or solids, integrated cable connection. Communications: HART (4 ... 20 mA) Bluetooth function: Enabled Cable length: 100m Process connection: 1-1/2\" NPT [(Taper), ASME B1.20.1]/ electrical connection 1\" NPT . . . Type of protection: Non Ex (ordinary locations) cFMus, cCSAus,CE, RCM . . ",1174,"ΤΕΜ",1,"PI1",1,"7ML53101EA060AA0"]
["7ML5310-1AB06-0AA0 ","SITRANS LR110 Radar level transmitter, continuous, non-contact, 15m (49.2ft) range, for liquids, slurries, or solids, integrated cable connection. Communications: HART (4 ... 20 mA) Bluetooth function: Enabled Cable length: 5m Process connection: R 1-1/2\" [(BSPT), EN 10226]/ electrical connection 1\" BSPT . Type of protection: Non Ex . . ",855,"ΤΕΜ",1,"PI1",1,"7ML53101AB060AA0"]
["7ML5310-1BB06-0AA0  ","SITRANS LR110 Radar level transmitter, continuous, non-contact, 15m (49.2ft) range, for liquids, slurries, or solids, integrated cable connection. Communications: HART (4 ... 20 mA) Bluetooth function: Enabled Cable length: 10m Process connection: R 1-1/2\" [(BSPT), EN 10226]/ electrical connection 1\" BSPT . . . Type of protection: Non Ex (ordinary locations) cFMus, cCSAus,CE, RCM . . ",872,"ΤΕΜ",1,"PI1",1,"7ML53101BB060AA0"]
["7ML5310-1CB06-0AA0","SITRANS LR110 Radar level transmitter, continuous, non-contact, 15m (49.2ft) range, for liquids, slurries, or solids, integrated cable connection. Communications: HART (4 ... 20 mA) Bluetooth function: Enabled Cable length: 30m Process connection: R 1-1/2\" [(BSPT), EN 10226]/ electrical connection 1\" BSPT Type of protection: Non Ex . . ",940,"ΤΕΜ",1,"PI1",1,"7ML53101CB060AA0"]
["7ML5310-1DB06-0AA0  ","SITRANS LR110 Radar level transmitter, continuous, non-contact, 15m (49.2ft) range, for liquids, slurries, or solids, integrated cable connection. Communications: HART (4 ... 20 mA) Bluetooth function: Enabled Cable length: 50m Process connection: R 1-1/2\" [(BSPT), EN 10226]/ electrical connection 1\" BSPT . Type of protection: Non Ex . . ",1007,"ΤΕΜ",1,"PI1",1,"7ML53101DB060AA0"]
["7ML5310-1EB06-0AA0  ","SITRANS LR110 Radar level transmitter, continuous, non-contact, 15m (49.2ft) range, for liquids, slurries, or solids, integrated cable connection. Communications: HART (4 ... 20 mA) Bluetooth function: Enabled Cable length: 100m Process connection: R 1-1/2\" [(BSPT), EN 10226]/ electrical connection 1\" BSPT . . . Type of protection: Non Ex (ordinary locations) cFMus, cCSAus,CE, RCM . . ",1174,"ΤΕΜ",1,"PI1",1,"7ML53101EB060AA0"]
["7ML5320-1AA06-0AH0","SITRANS LR120 Radar level transmitter, continuous, non-contact, 30 m (98.4 ft) range, for liquids slurries, and solids, integrated cable connection. Communications: HART (4 ... 20 mA) Bluetooth function: Enabled Cable length: 5m . . . . Type of protection: Non Ex (ordinary locations) cFMus, cCSAus,CE, RCM Electrical connection of the cable entry: 1\" BSPT . ",1077,"ΤΕΜ",1,"PI1",1,"7ML53201AA060AH0"]
["7ML5320-1BA06-0AH0","SITRANS LR120 Radar level transmitter, continuous, non-contact, 30 m (98.4 ft) range, for liquids slurries, and solids, integrated cable connection. Communications: HART (4 ... 20 mA) Bluetooth function: Enabled Cable length: 10m . . . . Type of protection: Non Ex (ordinary locations) cFMus, cCSAus,CE, RCM Electrical connection of the cable entry: 1\" BSPT . ",1094,"ΤΕΜ",1,"PI1",1,"7ML53201BA060AH0"]
["7ML5320-1CA06-0AH0","SITRANS LR120 Radar level transmitter, continuous, non-contact, 30 m (98.4 ft) range, for liquids slurries, and solids, integrated cable connection. Communications: HART (4 ... 20 mA) Bluetooth function: Enabled Cable length: 30m . . . . Type of protection: Non Ex (ordinary locations) cFMus, cCSAus,CE, RCM Electrical connection of the cable entry: 1\" BSPT . ",1161,"ΤΕΜ",1,"PI1",1,"7ML53201CA060AH0"]
["7ML5320-1DA06-0AH0","SITRANS LR120 Radar level transmitter, continuous, non-contact, 30 m (98.4 ft) range, for liquids slurries, and solids, integrated cable connection. Communications: HART (4 ... 20 mA) Bluetooth function: Enabled Cable length: 50m . . . . Type of protection: Non Ex (ordinary locations) cFMus, cCSAus,CE, RCM Electrical connection of the cable entry: 1\" BSPT . ",1228,"ΤΕΜ",1,"PI1",1,"7ML53201DA060AH0"]
["7ML5320-1EA06-0AH0"," SITRANS LR120 Radar level transmitter, continuous, non-contact, 30 m (98.4 ft) range, for liquids slurries, and solids, integrated cable connection. Communications: HART (4 ... 20 mA) Bluetooth function: Enabled Cable length: 100m . . . . Type of protection: Non Ex (ordinary locations) cFMus, cCSAus,CE, RCM Electrical connection of the cable entry: 1\" BSPT .",1395,"ΤΕΜ",1,"PI1",1,"7ML53201EA060AH0"]
["7ML5440-0AB00-0AA1"," SITRANS LR560 Radar level transmitter with flush lens antenna: continuous, non-contact, 100 m (328 ft) range, for general solids applications. Measurement and process temperature range: 40m (131 ft) max range, -40 C degrees to +100 C degrees Process connection: Universal flat-faced flange fits ANSI/DIN/JIS flanges: 3\" / 80 mm, 304 stainless steel Enclosure (with cable inlet): Stainless Steel, 1 X M20 x 1.5 (plastic gland included) . Label: Sitrans LR560 Pressure Rating: 0.5 bar g (7.5 psi g) maximum Output/communication: 4 to 20 mA, HART Approvals: General purpose, FM, CSA US/C, Industry Canada, FCC, CE, RED, RCM Local display interface: Without LDI (local display interface)",2636,"ΤΕΜ",1,"PI1",1,"7ML54400AB000AA1"]
["7ML5440-0AB00-0AC1"," SITRANS LR560 Radar level transmitter with flush lens antenna: continuous, non-contact, 100 m (328 ft) range, for general solids applications. Measurement and process temperature range: 40m (131 ft) max range, -40 C degrees to +100 C degrees Process connection: Universal flat-faced flange fits ANSI/DIN/JIS flanges: 3\" / 80 mm, 304 stainless steel Enclosure (with cable inlet): Stainless Steel, 1 X M20 x 1.5 (plastic gland included) . Label: Sitrans LR560 Pressure Rating: 0.5 bar g (7.5 psi g) maximum Output/communication: 4 to 20 mA, HART Approvals: ATEX II 1D, 1/2D, 2D, IECEx, 3G Ex nA/nL, CE, RED, RCM Local display interface: Without LDI (local display interface)",2758,"ΤΕΜ",1,"PI1",1,"7ML5440-0AB00-0AC1"]
["7ML5440-0AB00-0AA2"," SITRANS LR560 Radar level transmitter with flush lens antenna: continuous, non-contact, 100 m (328 ft) range, for general solids applications. Measurement and process temperature range: 40m (131 ft) max range, -40 C degrees to +100 C degrees Process connection: Universal flat-faced flange fits ANSI/DIN/JIS flanges: 3\" / 80 mm, 304 stainless steel Enclosure (with cable inlet): Stainless Steel, 1 X M20 x 1.5 (plastic gland included) . Label: Sitrans LR560 Pressure Rating: 0.5 bar g (7.5 psi g) maximum Output/communication: 4 to 20 mA, HART Approvals: General purpose, FM, CSA US/C, Industry Canada, FCC, CE, RED, RCM Local display interface: With LDI (local display interface)",2858,"ΤΕΜ",1,"PI1",1,"7ML54400AB000AA2"]
["7ML5440-0AB00-0AC2"," SITRANS LR560 Radar level transmitter with flush lens antenna: continuous, non-contact, 100 m (328 ft) range, for general solids applications. Measurement and process temperature range: 40m (131 ft) max range, -40 C degrees to +100 C degrees Process connection: Universal flat-faced flange fits ANSI/DIN/JIS flanges: 3\" / 80 mm, 304 stainless steel Enclosure (with cable inlet): Stainless Steel, 1 X M20 x 1.5 (plastic gland included) . Label: Sitrans LR560 Pressure Rating: 0.5 bar g (7.5 psi g) maximum Output/communication: 4 to 20 mA, HART Approvals: ATEX II 1D, 1/2D, 2D, IECEx, 3G Ex nA/nL, CE, RED, RCM Local display interface: With LDI (local display interface)",2979,"ΤΕΜ",1,"PI1",1,"7ML54400AB000AC2"]
["7ML5440-0BB00-0AA1"," SITRANS LR560 Radar level transmitter with flush lens antenna: continuous, non-contact, 100 m (328 ft) range, for general solids applications. Measurement and process temperature range: 40m (131 ft) max range, -40 C degrees to +100 C degrees Process connection: Universal flat-faced flange fits ANSI/DIN/JIS flanges: 4\" / 100 mm, 304 stainless steel Enclosure (with cable inlet): Stainless Steel, 1 X M20 x 1.5 (plastic gland included) . Label: Sitrans LR560 Pressure Rating: 0.5 bar g (7.5 psi g) maximum Output/communication: 4 to 20 mA, HART Approvals: General purpose, FM, CSA US/C, Industry Canada, FCC, CE, RED, RCM Local display interface: Without LDI (local display interface)",2758,"ΤΕΜ",1,"PI1",1,"7ML54400BB000AA1"]
["7ML5440-0BB00-0AC1"," SITRANS LR560 Radar level transmitter with flush lens antenna: continuous, non-contact, 100 m (328 ft) range, for general solids applications. Measurement and process temperature range: 40m (131 ft) max range, -40 C degrees to +100 C degrees Process connection: Universal flat-faced flange fits ANSI/DIN/JIS flanges: 4\" / 100 mm, 304 stainless steel Enclosure (with cable inlet): Stainless Steel, 1 X M20 x 1.5 (plastic gland included) . Label: Sitrans LR560 Pressure Rating: 0.5 bar g (7.5 psi g) maximum Output/communication: 4 to 20 mA, HART Approvals: ATEX II 1D, 1/2D, 2D, IECEx, 3G Ex nA/nL, CE, RED, RCM Local display interface: Without LDI (local display interface)",2879,"ΤΕΜ",1,"PI1",1,"7ML54400BB000AC1"]
["7ML5440-0BB00-0AA2"," SITRANS LR560 Radar level transmitter with flush lens antenna: continuous, non-contact, 100 m (328 ft) range, for general solids applications. Measurement and process temperature range: 40m (131 ft) max range, -40 C degrees to +100 C degrees Process connection: Universal flat-faced flange fits ANSI/DIN/JIS flanges: 4\" / 100 mm, 304 stainless steel Enclosure (with cable inlet): Stainless Steel, 1 X M20 x 1.5 (plastic gland included) . Label: Sitrans LR560 Pressure Rating: 0.5 bar g (7.5 psi g) maximum Output/communication: 4 to 20 mA, HART Approvals: General purpose, FM, CSA US/C, Industry Canada, FCC, CE, RED, RCM Local display interface: With LDI (local display interface)",2979,"ΤΕΜ",1,"PI1",1,"7ML54400BB000AA2"]
["7ML5440-0BB00-0AC2"," SITRANS LR560 Radar level transmitter with flush lens antenna: continuous, non-contact, 100 m (328 ft) range, for general solids applications. Measurement and process temperature range: 40m (131 ft) max range, -40 C degrees to +100 C degrees Process connection: Universal flat-faced flange fits ANSI/DIN/JIS flanges: 4\" / 100 mm, 304 stainless steel Enclosure (with cable inlet): Stainless Steel, 1 X M20 x 1.5 (plastic gland included) . Label: Sitrans LR560 Pressure Rating: 0.5 bar g (7.5 psi g) maximum Output/communication: 4 to 20 mA, HART Approvals: ATEX II 1D, 1/2D, 2D, IECEx, 3G Ex nA/nL, CE, RED, RCM Local display interface: With LDI (local display interface)",3100,"ΤΕΜ",1,"PI1",1,"7ML54400BB000AC2"]
["7ML5440-0GB00-0AA1"," SITRANS LR560 Radar level transmitter with flush lens antenna: continuous, non-contact, 100 m (328 ft) range, for general solids applications. Measurement and process temperature range: 40m (131 ft) max range, -40 C degrees to +100 C degrees Process connection: Universal flat-faced flange fits ANSI/DIN/JIS flanges: 3\" / 80 mm, painted aluminum, with integral aimer Enclosure (with cable inlet): Stainless Steel, 1 X M20 x 1.5 (plastic gland included) . Label: Sitrans LR560 Pressure Rating: 0.5 bar g (7.5 psi g) maximum Output/communication: 4 to 20 mA, HART Approvals: General purpose, FM, CSA US/C, Industry Canada, FCC, CE, RED, RCM Local display interface: Without LDI (local display interface)",2636,"ΤΕΜ",1,"PI1",1,"7ML54400GB000AA1"]
["7ML5440-0GB00-0AC1"," SITRANS LR560 Radar level transmitter with flush lens antenna: continuous, non-contact, 100 m (328 ft) range, for general solids applications. Measurement and process temperature range: 40m (131 ft) max range, -40 C degrees to +100 C degrees Process connection: Universal flat-faced flange fits ANSI/DIN/JIS flanges: 3\" / 80 mm, painted aluminum, with integral aimer Enclosure (with cable inlet): Stainless Steel, 1 X M20 x 1.5 (plastic gland included) . Label: Sitrans LR560 Pressure Rating: 0.5 bar g (7.5 psi g) maximum Output/communication: 4 to 20 mA, HART Approvals: ATEX II 1D, 1/2D, 2D, IECEx, 3G Ex nA/nL, CE, RED, RCM Local display interface: Without LDI (local display interface)",2758,"ΤΕΜ",1,"PI1",1,"7ML54400GB000AC1"]
["7ML5440-0GB00-0AA2"," SITRANS LR560 Radar level transmitter with flush lens antenna: continuous, non-contact, 100 m (328 ft) range, for general solids applications. Measurement and process temperature range: 40m (131 ft) max range, -40 C degrees to +100 C degrees Process connection: Universal flat-faced flange fits ANSI/DIN/JIS flanges: 3\" / 80 mm, painted aluminum, with integral aimer Enclosure (with cable inlet): Stainless Steel, 1 X M20 x 1.5 (plastic gland included) . Label: Sitrans LR560 Pressure Rating: 0.5 bar g (7.5 psi g) maximum Output/communication: 4 to 20 mA, HART Approvals: General purpose, FM, CSA US/C, Industry Canada, FCC, CE, RED, RCM Local display interface: With LDI (local display interface)",2858,"ΤΕΜ",1,"PI1",1,"7ML54400GB000AA2"]
["7ML5440-0GB00-0AC2"," SITRANS LR560 Radar level transmitter with flush lens antenna: continuous, non-contact, 100 m (328 ft) range, for general solids applications. Measurement and process temperature range: 40m (131 ft) max range, -40 C degrees to +100 C degrees Process connection: Universal flat-faced flange fits ANSI/DIN/JIS flanges: 3\" / 80 mm, painted aluminum, with integral aimer Enclosure (with cable inlet): Stainless Steel, 1 X M20 x 1.5 (plastic gland included) . Label: Sitrans LR560 Pressure Rating: 0.5 bar g (7.5 psi g) maximum Output/communication: 4 to 20 mA, HART Approvals: ATEX II 1D, 1/2D, 2D, IECEx, 3G Ex nA/nL, CE, RED, RCM Local display interface: With LDI (local display interface)",2979,"ΤΕΜ",1,"PI1",1,"7ML54400GB000AC2"]
["7ML5440-0HB00-0AA1"," SITRANS LR560 Radar level transmitter with flush lens antenna: continuous, non-contact, 100 m (328 ft) range, for general solids applications. Measurement and process temperature range: 40m (131 ft) max range, -40 C degrees to +100 C degrees Process connection: Universal flat-faced flange fits ANSI/DIN/JIS flanges: 4\" / 100 mm, painted aluminum, with integral aimer Enclosure (with cable inlet): Stainless Steel, 1 X M20 x 1.5 (plastic gland included) . Label: Sitrans LR560 Pressure Rating: 0.5 bar g (7.5 psi g) maximum Output/communication: 4 to 20 mA, HART Approvals: General purpose, FM, CSA US/C, Industry Canada, FCC, CE, RED, RCM Local display interface: Without LDI (local display interface)",2758,"ΤΕΜ",1,"PI1",1,"7ML54400HB000AA1"]
["7ML5440-0HB00-0AC1"," SITRANS LR560 Radar level transmitter with flush lens antenna: continuous, non-contact, 100 m (328 ft) range, for general solids applications. Measurement and process temperature range: 40m (131 ft) max range, -40 C degrees to +100 C degrees Process connection: Universal flat-faced flange fits ANSI/DIN/JIS flanges: 4\" / 100 mm, painted aluminum, with integral aimer Enclosure (with cable inlet): Stainless Steel, 1 X M20 x 1.5 (plastic gland included) . Label: Sitrans LR560 Pressure Rating: 0.5 bar g (7.5 psi g) maximum Output/communication: 4 to 20 mA, HART Approvals: ATEX II 1D, 1/2D, 2D, IECEx, 3G Ex nA/nL, CE, RED, RCM Local display interface: Without LDI (local display interface)",2879,"ΤΕΜ",1,"PI1",1,"7ML54400HB000AC1"]
["7ML5440-0HB00-0AA2"," SITRANS LR560 Radar level transmitter with flush lens antenna: continuous, non-contact, 100 m (328 ft) range, for general solids applications. Measurement and process temperature range: 40m (131 ft) max range, -40 C degrees to +100 C degrees Process connection: Universal flat-faced flange fits ANSI/DIN/JIS flanges: 4\" / 100 mm, painted aluminum, with integral aimer Enclosure (with cable inlet): Stainless Steel, 1 X M20 x 1.5 (plastic gland included) . Label: Sitrans LR560 Pressure Rating: 0.5 bar g (7.5 psi g) maximum Output/communication: 4 to 20 mA, HART Approvals: General purpose, FM, CSA US/C, Industry Canada, FCC, CE, RED, RCM Local display interface: With LDI (local display interface)",2979,"ΤΕΜ",1,"PI1",1,"7ML54400HB000AA2"]
["7ML5440-0HB00-0AC2"," SITRANS LR560 Radar level transmitter with flush lens antenna: continuous, non-contact, 100 m (328 ft) range, for general solids applications. Measurement and process temperature range: 40m (131 ft) max range, -40 C degrees to +100 C degrees Process connection: Universal flat-faced flange fits ANSI/DIN/JIS flanges: 4\" / 100 mm, painted aluminum, with integral aimer Enclosure (with cable inlet): Stainless Steel, 1 X M20 x 1.5 (plastic gland included) . Label: Sitrans LR560 Pressure Rating: 0.5 bar g (7.5 psi g) maximum Output/communication: 4 to 20 mA, HART Approvals: ATEX II 1D, 1/2D, 2D, IECEx, 3G Ex nA/nL, CE, RED, RCM Local display interface: With LDI (local display interface)",3100,"ΤΕΜ",1,"PI1",1,"7ML54400HB000AC2"]
["7ML1930-1BK"," Hand Programmer, Intrinsically safe, EEx ia (LUI version)",189,"ΤΕΜ",1,"PI1",1,"7ML19301BK"]
["7ML1930-1FJ","Local user interface",259,"ΤΕΜ",1,"PI1",1,"7ML19301FJ"]
["7ML1930-1FK","Sun shield cover",178,"ΤΕΜ",1,"PI1",1,"7ML19301FK"]
["6DR5010-0NG00-0AA0","SIPART PS2 smart electropneumatic positioner for pneumatic linear and part-turn actuators; 2-wire; 4...20mA; single action; polycarbonate enclosure . Without explosion protection Connection thread el.: M20x1.5 / pneu.: G 1/4 Without Without . Brief instructions German / English / Chinese Standard / Fail-Safe - Depressurizing the actuator in case of failure of electrical auxiliary power Without ",922,"ΤΕΜ",1,"PI3",1,"6DR50100NG000AA0"]
["6DR5010-0EG00-0AA0","SIPART PS2 smart electropneumatic positioner for pneumatic linear and part-turn actuators; 2-wire; 4...20mA; single action; polycarbonate enclosure . Type of protection (Ex): Intrinsic safety (Ex i) Connection thread el.: M20x1.5 / pneu.: G 1/4 Without Without . Brief instructions German / English / Chinese Standard / Fail-Safe - Depressurizing the actuator in case of failure of electrical auxiliary power Without ",998,"ΤΕΜ",1,"PI3",1,"6DR50100EG000AA0"]
["6DR5020-0NG00-0AA0","SIPART PS2 smart electropneumatic positioner for pneumatic linear and part-turn actuators; 2-wire; 4...20mA; double action; polycarbonate enclosure . Without explosion protection Connection thread el.: M20x1.5 / pneu.: G 1/4 Without Without . Brief instructions German / English / Chinese Standard / Fail-Safe - Depressurizing the actuator in case of failure of electrical auxiliary power without mounted pressure gauge block ",1060,"ΤΕΜ",1,"PI3",1,"6DR50200NG000AA0"]
["6DR5020-0EG00-0AA0","SIPART PS2 smart electropneumatic positioner for pneumatic linear and part-turn actuators; 2-wire; 4...20mA; double action; polycarbonate enclosure Connection thread el.: M20x1.5 Without Without . Brief instructions German / without mounted pressure gauge ",1136,"ΤΕΜ",1,"PI3",1,"6DR50200EG000AA0"]
["6DR5110-0NG00-0AA0","SIPART PS2 smart electropneumatic positioner for pneumatic linear and part-turn actuators; 2-wire; 4...20mA with HART-interface; single action; polycarbonate enclosure . Without explosion protection Connection thread el.: M20x1.5 / pneu.: G 1/4 Without Without . Brief instructions German / English / Chinese Standard / Fail-Safe - Depressurizing the actuator in case of failure of electrical auxiliary power without mounted pressure gauge block ",1099,"ΤΕΜ",1,"PI3",1,"6DR51100NG000AA0"]
["6DR5120-0NG00-0AA0","SIPART PS2 smart electropneumatic positioner for pneumatic linear and part-turn actuators; 2-wire; 4...20mA with HART-interface; double action; polycarbonate enclosure . Without explosion protection Connection thread el.: M20x1.5 / pneu.: G 1/4 Without Without . Brief instructions German / English / Chinese Standard / Fail-Safe - Depressurizing the actuator in case of failure of electrical auxiliary power without mounted pressure gauge block ",1235,"ΤΕΜ",1,"PI3",1,"6DR51200NG000AA0"]
["6DR5310-0NG00-0AA0","SIPART PS2 smart electropneumatic positioner for pneumatic linear and part-turn actuators; 2-,3-,4-wire; 4...20mA; single action; polycarbonate enclosure . Without explosion protection Connection thread el.: M20x1.5 / pneu.: G 1/4 Without Without . Brief instructions German / English / Chinese Standard / Fail-Safe - Depressurizing the actuator in case of failure of electrical auxiliary power without mounted pressure gauge block ",969,"ΤΕΜ",1,"PI3",1,"6DR53100NG000AA0"]
["6DR5320-0NG00-0AA0","SIPART PS2 smart electropneumatic positioner for pneumatic linear and part-turn actuators; 2-,3-,4-wire; 4...20mA; double action; polycarbonate enclosure . Without explosion protection Connection thread el.: M20x1.5 / pneu.: G 1/4 Without Without . Brief instructions German / English / Chinese Standard / Fail-Safe - Depressurizing the actuator in case of failure of electrical auxiliary power without mounted pressure gauge block ",1106,"ΤΕΜ",1,"PI3",1,"6DR53200NG000AA0"]
["6DR5210-0EG00-0AA0","SIPART PS2 smart electropneumatic positioner for pneumatic linear and part-turn actuators; 2-,3-,4-wire; 4...20mA with HART-interface; single action; polycarbonate enclosure . Type of protection (Ex): Intrinsic safety (Ex i) Connection thread el.: M20x1.5 / pneu.: G 1/4 Without Without . Brief instructions German / English / Chinese Standard / Fail-Safe - Depressurizing the actuator in case of failure of electrical auxiliary power without mounted pressure gauge block ",1192,"ΤΕΜ",1,"PI3",1,"6DR52100EG000AA0"]
["6DR5220-0EG00-0AA0","SIPART PS2 smart electropneumatic positioner for pneumatic linear and part-turn actuators; 2-,3-,4-wire; 4...20mA with HART-interface; double action; polycarbonate enclosure . Type of protection (Ex): Intrinsic safety (Ex i) Connection thread el.: M20x1.5 / pneu.: G 1/4 Without Without . Brief instructions German / English / Chinese Standard / Fail-Safe - Depressurizing the actuator in case of failure of electrical auxiliary power without mounted pressure gauge block ",1331,"ΤΕΜ",1,"PI3",1,"6DR52200EG000AA0"]
["6DR5510-0NG00-0AA0","SIPART PS2 smart electropneumatic positioner for pneumatic linear and part-turn actuators; PROFIBUS-PA operation; single action; polycarbonate enclosure . Without explosion protection Connection thread el.: M20x1.5 / pneu.: G 1/4 Without Without . Brief instructions German / English / Chinese Standard / Fail-Safe - Depressurizing the actuator in case of failure of electrical auxiliary power without mounted pressure gauge block ",1281,"ΤΕΜ",1,"PI3",1,"6DR55100NG000AA0"]
["6DR5510-0EG00-0AA0","SIPART PS2 smart electropneumatic positioner for pneumatic linear and part-turn actuators; PROFIBUS-PA operation; single action; polycarbonate enclosure . Type of protection (Ex): Intrinsic safety (Ex i) Connection thread el.: M20x1.5 / pneu.: G 1/4 Without Without . Brief instructions German / English / Chinese Standard / Fail-Safe - Depressurizing the actuator in case of failure of electrical auxiliary power without mounted pressure gauge block ",1357,"ΤΕΜ",1,"PI3",1,"6DR55100EG000AA0"]
["6DR5520-0NG00-0AA0","SIPART PS2 smart electropneumatic positioner for pneumatic linear and part-turn actuators; PROFIBUS-PA operation; double action; polycarbonate enclosure . Without explosion protection Connection thread el.: M20x1.5 / pneu.: G 1/4 Without Without . Brief instructions German / English / Chinese Standard / Fail-Safe - Depressurizing the actuator in case of failure of electrical auxiliary power without mounted pressure gauge block ",1418,"ΤΕΜ",1,"PI3",1,"6DR55200NG000AA0"]
["6DR5520-0EG00-0AA0","SIPART PS2 smart electropneumatic positioner for pneumatic linear and part-turn actuators; PROFIBUS-PA operation; double action; polycarbonate enclosure . Type of protection (Ex): Intrinsic safety (Ex i) Connection thread el.: M20x1.5 / pneu.: G 1/4 Without Without . Brief instructions German / English / Chinese Standard / Fail-Safe - Depressurizing the actuator in case of failure of electrical auxiliary power without mounted pressure gauge block ",1494,"ΤΕΜ",1,"PI3",1,"6DR55200EG000AA0"]
["6DR4004-8J","Iy module plug-in module for analog current output signal for SIPART PS2 electropneumatic positioner, position feedback, signal current 4-20 mA, simple to retrofit, not explosion-proof ",279,"ΤΕΜ",1,"PI3",1,"6DR40048J"]
["6DR4004-6J","Iy module plug-in module for analog current output signal for SIPART PS2 electropneumatic positioner, position feedback, signal current 4-20 mA, simple to retrofit, with explosion protection: eexib ",300,"ΤΕΜ",1,"PI3",1,"6DR40046J"]
["6DR4004-8A","Alarm module . plug-in module for binary signals for SIPART PS2 electropneumatic positioner, simple to retrofit, 2 limit outputs min. or max., 1 fault output, 1 binary input, not explosion-proof ",211,"ΤΕΜ",1,"PI3",1,"6DR40048A"]
["6DR4004-6A","Alarm module . plug-in module for binary signals for SIPART PS2 electropneumatic positioner, simple to retrofit, 2 limit outputs min. or max., 1 fault output, 1 binary input, with explosion protection: eexib ",231,"ΤΕΜ",1,"PI3",1,"6DR40046A"]
["6DR4004-8NN20"," NCS-sensor for SIPART PS2 for non-contacting detection of position without explosion-proof . Cable length 6 m (19.68 ft) for linear actuators up to 14mm (mounted with individual mounting solution) Manual in german and english",360,"ΤΕΜ",1,"PI3",1,"6DR40048NN20"]
["6DR4004-6NN20"," NCS-sensor for SIPART PS2 for non-contacting detection of position with explosion-proof . Cable length 6 m (19.68 ft) for linear actuators up to 14mm (mounted with individual mounting solution) Manual in german and english",378,"ΤΕΜ",1,"PI3",1,"6DR40046NN20"]
["6DR4004-8NN30","NCS-sensor for SIPART PS2 for non-contacting detection of position without explosion-proof . Cable length 6 m (19.68 ft) for linear actuators > 14mm Manual in german and english ",640,"ΤΕΜ",1,"PI3",1,"6DR40048NN30"]
["6DR4004-6NN30"," NCS-sensor for SIPART PS2 for non-contacting detection of position with explosion-proof . Cable length 6 m (19.68 ft) for linear actuators > 14mm Manual in german and english",658,"ΤΕΜ",1,"PI3",1,"6DR40046NN30"]
["6DR4004-1M","MANOMETER MANIFOLD FOR SIPART PS2 ELECTROPNEUMATIC POSITIONER 6DR40**-1*, SINGLE ACTION, SIMPLE TO RETROFIT 1 NETWORK PRESSURE MANOM: 10BAR 1 CHAMBER PRESSURE MANOM: 6BAR ",149,"ΤΕΜ",1,"PI3",1,"6DR40041M"]
["6DR4004-2M","Manometer manifold for for SIPART PS 2 electropneumatic positioner double action simple to retrofit 1 network pressure manom:10BAR 2 chamber pressure manom: 6BAR ",173,"ΤΕΜ",1,"PI3",1,"6DR40042M"]
["6DR4004-8D","Mounting kit for SIPART PS2 for part-turn actuator to VDI/VDE 3845 (NAMUR) plastic coupling wheel ",76,"ΤΕΜ",1,"PI3",1,"6DR40048D"]
["6DR4004-1D","SIPART PS2 CONSOLE FOR NAMUR ASSEMBLY WITH ROTARY ACTUATORS 80 X 30 X 20 MM ",62,"ΤΕΜ",1,"PI3",1,"6DR40041D"]
["6DR4004-2D","SIPART PS2 CONSOLE FOR NAMUR ASSEMBLY WITH ROTARY ACTUATORS 80 X 30 X 30 MM ",74,"ΤΕΜ",1,"PI3",1,"6DR40042D"]
["6DR4004-3D","SIPART PS2 CONSOLE FOR NAMUR ASSEMBLY WITH ROTARY ACTUATORS 130 X 30 X 30 MM ",86,"ΤΕΜ",1,"PI3",1,"6DR40043D"]
["6DR4004-4D","SIPART PS2 CONSOLE FOR NAMUR ASSEMBLY WITH ROTARY ACTUATORS 130 X 30 X 50 MM ",94,"ΤΕΜ",1,"PI3",1,"6DR40044D"]
["6DR4004-8V","Mounting kit for SIPART PS 2",97,"ΤΕΜ",1,"PI3",1,"6DR40048V"]
["6DR4004-8L","LEVER FOR MOUNTING SET 6DR4004-8V OF SIPART PS2 ELECTROPNEUMATIC POSITIONER TO IEC 534 PART 6 TRAVEL RANGES: 35-130 MM, VA STEEL (NIRO) ",30,"ΤΕΜ",1,"PI3",1,"6DR40048L"]
["6DR4004-8VK","MOUNTING SET FOR SIPART PS2 ELECTROPNEUMATIC POSITIONER MOUNTING ON LINEAR ACTUATORS CONSTING OF A SHORT LEVER (COMPLETE MOUNTED) AND PICK- UP BRACKET, CLAMPING PIECES (ALUMINIUM) ASSEMBLY AND SCREWS. STRAKE RANGES: 2MM-35MM, OTHER METAL PARTS VA-STEEL. ",60,"ΤΕΜ",1,"PI3",1,"6DR40048VK"]
["6DR4004-8VL","MOUNTING SET FOR SIPART PS2 ELECTROPNEUMATIC POSITIONER MOUNTING ON LINEAR ACTUATORS CONSISTING OF A LONG LEVER (COMPLETE MOUNTED) AND PICK- UP BRACKET, CLAMPING ASSEMBLY AND SCREWS. STRAKE RANGES: 30MM-130MM METAL PARTS VA-STEEL. ",60,"ΤΕΜ",1,"PI3",1,"6DR40048VL"]
["6DR4004-8K","MECHANICAL LIMIT SWITCH MODULE, WITH GALVANICAL SWITCH CONTACTS, FOR ELECTROPNEUMATIC POSITIONER SIPART PS2, TO RETROFIT, 1 FAULT OUTPUT, NOT EXPLOSION PROOF Not suitable for natural gas operation! ",258,"ΤΕΜ",1,"PI3",1,"6DR40048K"]
["6DR4004-6K","MECHANICAL LIMIT SWITCH MODULE, WITH GALVANICAL SWITCH CONTACTS, FOR ELECTROPNEUMATIC POSITIONER SIPART PS2, TO RETROFIT, 1 FAULT OUTPUT, EXPLOSION PROOF TO ATEX AND FM Not suitable for natural gas operation! ******************************* Attention: only Ex ia/ib to ATEX and FM certified, CSA:on request! ******************************* ",289,"ΤΕΜ",1,"PI3",1,"6DR40046K"]
["6DR4004-8G","SIA module, with slot-type initiators for electropneumatic positioner SIPART PS2, to retrofit, 1 fault output, not explosion proof ",445,"ΤΕΜ",1,"PI3",1,"6DR40048G"]
["6DR4004-6G","SIA module, with slot-type initiators for electropneumatic positioner SIPART PS2, to retrofit, 1 fault output, with explosion proof Eex IA/IB ",459,"ΤΕΜ",1,"PI3",1,"6DR40046G"]
["7MH7560-1AA01","Sitrans AS100: acoustic sensor for flow detection. It can warn of changes to material flow to prevent costly damage or downtime. Sensor: Standard temperature range (-20 C to +80 C) Cable length: 4 meters (13.12 ft) Sensor mounting: none . Approvals: CE,RCM,EAC,KCC ",1110,"ΤΕΜ",1,"PI3",1,"7MH75601AA01"]
["7MH7560-1AA05","Sitrans AS100: acoustic sensor for flow detection. It can warn of changes to material flow to prevent costly damage or downtime. Sensor: Standard temperature range (-20 C to +80 C) Cable length: 4 meters (13.12 ft) Sensor mounting: none . Approvals: CE,RCM,FM/CSA Class II Div. I, Groups E,F and G, ATEX II 3D, c/w M20 female adaptor EAC Ex ",1290,"ΤΕΜ",1,"PI3",1,"7MH75601AA05"]
["7MH7560-3AA01","Sitrans AS100: acoustic sensor for flow detection. It can warn of changes to material flow to prevent costly damage or downtime. Sensor: Extended temperature range (-40 C to +125 C) Cable length: 4 meters (13.12 ft) Sensor mounting: none . Approvals: CE,RCM,EAC,KCC ",1458,"ΤΕΜ",1,"PI3",1,"7MH75603AA01"]
["7MH7562-4AA","SITRANS CU02 Control unit: set-point alarm controller, for use with AS100 acoustic sensor. Input voltage: 230 V AC Enclosure: Standard DIN Rail Approvals: CSA,CE,RCM,EAC,KCC ",709,"ΤΕΜ",1,"PI3",1,"7MH75624AA"]
["7MH7701-0AA00-0A","Motion Failure Alarm MFA, DSD, NCT A highly sensitive dual setpoint motion sensor system, used with up to 2 MSP and XPP probes. Capable of hi/lo setpoint as well as differential monitoring with 2 additional probes. ",502,"ΤΕΜ",1,"PI3",1,"7MH77010AA000A"]
["7MH7702-0B","Remote Mounted Amplifier RMA Remote mounted amplifier for 2 Milltronics MSP-1, MSP-3, MSP-9, MSP-12 and XPP-5 motion sensing probes ",325,"ΤΕΜ",1,"PI3",1,"7MH77020B"]
["7MH7146-0EA","Milltronics Motion sensing probes: heavy duty, 100 mm measuring range, for use with RMA, MFA 4p, WM300 MFA, or other control. Cable length: Standard length (per notes in model section) Model: MSP-12, 1/2\" NPT cable inlet no cable Approval: CE,RCM,EAC,KCC ",413,"ΤΕΜ",1,"PI3",1,"7MH71460EA"]
["7ML5740-1AA01-0A","The SITRANS RD200 is a universal input, panel mount remote digital display for process instrumentation. RD200 85-265 VAC remote display ",322,"ΤΕΜ",1,"PI1",1,"7ML57401AA010A"]
["7ML5740-1AB01-0A","The SITRANS RD200 is a universal input, panel mount remote digital display for process instrumentation. RD200 85-265 VAC DISPLAY with 2 Relays ",403,"ΤΕΜ",1,"PI1",1,"7ML57401AB010A"]
["7ML5740-1AC01-0A","The SITRANS RD200 is a universal input, panel mount remote digital display for process instrumentation. RD200 85-265 VAC DISPLAY with 4-20 mA Output ",464,"ΤΕΜ",1,"PI1",1,"7ML57401AC010A"]
["7ML5740-1BA01-0A","The SITRANS RD200 is a universal input, panel mount remote digital display for process instrumentation. RD200 85-265 VAC DISPLAY with 24V Supply ",376,"ΤΕΜ",1,"PI1",1,"7ML57401BA010A"]
["7ML5740-1BB01-0A","The SITRANS RD200 is a universal input, panel mount remote digital display for process instrumentation. RD200 85-265 VAC DISPLAY with 2 Relays and 24V Supply ",471,"ΤΕΜ",1,"PI1",1,"7ML57401BB010A"]
["7ML5740-1BC01-0A","The SITRANS RD200 is a universal input, panel mount remote digital display for process instrumentation. RD200 85-265 VAC DISPLAY with 4-20 and 24V Supply ",532,"ΤΕΜ",1,"PI1",1,"7ML57401BC010A"]
["7ML5740-2AA01-0A","The SITRANS RD200 is a universal input, panel mount remote digital display for process instrumentation. RD200 12-36 VDC DISPLAY ",391,"ΤΕΜ",1,"PI1",1,"7ML57402AA010A"]
["7ML5740-2AB01-0A","The SITRANS RD200 is a universal input, panel mount remote digital display for process instrumentation. RD200 12-36 VDC Display with 2 Relays ",484,"ΤΕΜ",1,"PI1",1,"7ML57402AB010A"]
["7ML5740-2AC01-0A","The SITRANS RD200 is a universal input, panel mount remote digital display for process instrumentation. RD200 12-36 VDC Display with 4-20 mA Output ",544,"ΤΕΜ",1,"PI1",1,"7ML57402AC010A"]
["7ML5744-1AA00-0A","SITRANS RD300 Display: remote digital panel mount process display with current or voltage inputs. Two input, multi-line display, totalizer and pump control. Input voltage: 85 ... 265 V AC,50/60 Hz; 90 ... 265 V DC, 20 W max Output: None Type: Single input process and flow rate totalizer Meter Display: Standard Approvals: UL & C-UL & CE . . ",551,"ΤΕΜ",1,"PI1",1,"7ML57441AA000A"]
["7ML5744-1BA00-0A","SITRANS RD300 Display: remote digital panel mount process display with current or voltage inputs. Two input, multi-line display, totalizer and pump control. Input voltage: 85 ... 265 V AC,50/60 Hz; 90 ... 265 V DC, 20 W max Output: 2 Relays Type: Single input process and flow rate totalizer Meter Display: Standard Approvals: UL & C-UL & CE . . ",617,"ΤΕΜ",1,"PI1",1,"7ML57441BA000A"]
["7ML5744-1CA00-0A","SITRANS RD300 Display: remote digital panel mount process display with current or voltage inputs. Two input, multi-line display, totalizer and pump control. Input voltage: 85 ... 265 V AC,50/60 Hz; 90 ... 265 V DC, 20 W max Output: 4 Relays Type: Single input process and flow rate totalizer Meter Display: Standard Approvals: UL & C-UL & CE . . ",680,"ΤΕΜ",1,"PI1",1,"7ML57441CA000A"]
["7ML5744-1DA00-0A  ","SITRANS RD300 Display: remote digital panel mount process display with current or voltage inputs. Two input, multi-line display, totalizer and pump control. Input voltage: 85 ... 265 V AC,50/60 Hz; 90 ... 265 V DC, 20 W max Output: 4 ... 20 mA output Type: Single input process and flow rate totalizer Meter Display: Standard Approvals: UL & C-UL & CE . . ",647,"ΤΕΜ",1,"PI1",1,"7ML57441DA000A"]
["7ML5744-1EA00-0A  ","SITRANS RD300 Display: remote digital panel mount process display with current or voltage inputs. Two input, multi-line display, totalizer and pump control. Input voltage: 85 ... 265 V AC,50/60 Hz; 90 ... 265 V DC, 20 W max Output: 2 Relays and 4 ... 20 mA output Type: Single input process and flow rate totalizer Meter Display: Standard Approvals: UL & C-UL & CE . . ",708,"ΤΕΜ",1,"PI1",1,"7ML57441EA000A"]
["7ML5744-1FA00-0A  ","SITRANS RD300 Display: remote digital panel mount process display with current or voltage inputs. Two input, multi-line display, totalizer and pump control. Input voltage: 85 ... 265 V AC,50/60 Hz; 90 ... 265 V DC, 20 W max Output: 4 Relays and 4 ... 20 mA output Type: Single input process and flow rate totalizer Meter Display: Standard Approvals: UL & C-UL & CE . . ",777,"ΤΕΜ",1,"PI1",1,"7ML57441FA000A"]
["7ML5744-1AB00-0A"," SITRANS RD300 Display: remote digital panel mount process display with current or voltage inputs. Two input, multi-line display, totalizer and pump control. Input voltage: 85 ... 265 V AC,50/60 Hz; 90 ... 265 V DC, 20 W max Output: None Type: Dual input process Meter Display: Standard Approvals: UL & C-UL & CE . .",702,"ΤΕΜ",1,"PI1",1,"7ML57441AB000A"]
["7ML5744-1BB00-0A","SITRANS RD300 Display: remote digital panel mount process display with current or voltage inputs. Two input, multi-line display, totalizer and pump control. Input voltage: 85 ... 265 V AC,50/60 Hz; 90 ... 265 V DC, 20 W max Output: 2 Relays Type: Dual input process Meter Display: Standard Approvals: UL & C-UL & CE . . ",769,"ΤΕΜ",1,"PI1",1,"7ML57441BB000A"]
["7ML5744-1CB00-0A","SITRANS RD300 Display: remote digital panel mount process display with current or voltage inputs. Two input, multi-line display, totalizer and pump control. Input voltage: 85 ... 265 V AC,50/60 Hz; 90 ... 265 V DC, 20 W max Output: 4 Relays Type: Dual input process Meter Display: Standard Approvals: UL & C-UL & CE . . ",832,"ΤΕΜ",1,"PI1",1,"7ML57441CB000A"]
["7ML5744-1DB00-0A  ","SITRANS RD300 Display: remote digital panel mount process display with current or voltage inputs. Two input, multi-line display, totalizer and pump control. Input voltage: 85 ... 265 V AC,50/60 Hz; 90 ... 265 V DC, 20 W max Output: 4 ... 20 mA output Type: Dual input process Meter Display: Standard Approvals: UL & C-UL & CE . . ",799,"ΤΕΜ",1,"PI1",1,"7ML57441DB000A"]
["7ML5744-1EB00-0A  ","SITRANS RD300 Display: remote digital panel mount process display with current or voltage inputs. Two input, multi-line display, totalizer and pump control. Input voltage: 85 ... 265 V AC,50/60 Hz; 90 ... 265 V DC, 20 W max Output: 2 Relays and 4 ... 20 mA output Type: Dual input process Meter Display: Standard Approvals: UL & C-UL & CE . . ",859,"ΤΕΜ",1,"PI1",1,"7ML57441EB000A"]
["7ML5744-1FB00-0A  ","SITRANS RD300 Display: remote digital panel mount process display with current or voltage inputs. Two input, multi-line display, totalizer and pump control. Input voltage: 85 ... 265 V AC,50/60 Hz; 90 ... 265 V DC, 20 W max Output: 4 Relays and 4 ... 20 mA output Type: Dual input process Meter Display: Standard Approvals: UL & C-UL & CE . . ",928,"ΤΕΜ",1,"PI1",1,"7ML57441FB000A"]
["7ML5744-2AA00-0A","SITRANS RD300 Display: remote digital panel mount process display with current or voltage inputs. Two input, multi-line display, totalizer and pump control. Input voltage: 12 ... 36 V DC; 12 ... 24 V AC, 6 W max. Output: None Type: Single input process and flow rate totalizer Meter Display: Standard Approvals: UL & C-UL & CE . . ",647,"ΤΕΜ",1,"PI1",1,"7ML57442AA000A"]
["7ML5744-2BA00-0A","SITRANS RD300 Display: remote digital panel mount process display with current or voltage inputs. Two input, multi-line display, totalizer and pump control. Input voltage: 12 ... 36 V DC; 12 ... 24 V AC, 6 W max. Output: 2 Relays Type: Single input process and flow rate totalizer Meter Display: Standard Approvals: UL & C-UL & CE . . ",714,"ΤΕΜ",1,"PI1",1,"7ML57442BA000A"]
["7ML5744-2CA00-0A","SITRANS RD300 Display: remote digital panel mount process display with current or voltage inputs. Two input, multi-line display, totalizer and pump control. Input voltage: 12 ... 36 V DC; 12 ... 24 V AC, 6 W max. Output: 4 Relays Type: Single input process and flow rate totalizer Meter Display: Standard Approvals: UL & C-UL & CE . . ",777,"ΤΕΜ",1,"PI1",1,"7ML57442CA000A"]
["7ML5744-2DA00-0A  ","SITRANS RD300 Display: remote digital panel mount process display with current or voltage inputs. Two input, multi-line display, totalizer and pump control. Input voltage: 12 ... 36 V DC; 12 ... 24 V AC, 6 W max. Output: 4 ... 20 mA output Type: Single input process and flow rate totalizer Meter Display: Standard Approvals: UL & C-UL & CE . . ",744,"ΤΕΜ",1,"PI1",1,"7ML57442DA000A"]
["7ML5744-2EA00-0A  ","SITRANS RD300 Display: remote digital panel mount process display with current or voltage inputs. Two input, multi-line display, totalizer and pump control. Input voltage: 12 ... 36 V DC; 12 ... 24 V AC, 6 W max. Output: 2 Relays and 4 ... 20 mA output Type: Single input process and flow rate totalizer Meter Display: Standard Approvals: UL & C-UL & CE . . ",805,"ΤΕΜ",1,"PI1",1,"7ML57442EA000A"]
["7ML5744-2FA00-0A  ","SITRANS RD300 Display: remote digital panel mount process display with current or voltage inputs. Two input, multi-line display, totalizer and pump control. Input voltage: 12 ... 36 V DC; 12 ... 24 V AC, 6 W max. Output: 4 Relays and 4 ... 20 mA output Type: Single input process and flow rate totalizer Meter Display: Standard Approvals: UL & C-UL & CE . . ",873,"ΤΕΜ",1,"PI1",1,"7ML57442FA000A"]
["7ML5744-2AB00-0A","SITRANS RD300 Display: remote digital panel mount process display with current or voltage inputs. Two input, multi-line display, totalizer and pump control. Input voltage: 12 ... 36 V DC; 12 ... 24 V AC, 6 W max. Output: None Type: Dual input process Meter Display: Standard Approvals: UL & C-UL & CE . . ",799,"ΤΕΜ",1,"PI1",1,"7ML57442AB000A"]
["7ML5744-2BB00-0A"," SITRANS RD300 Display: remote digital panel mount process display with current or voltage inputs. Two input, multi-line display, totalizer and pump control. Input voltage: 12 ... 36 V DC; 12 ... 24 V AC, 6 W max. Output: 2 Relays Type: Dual input process Meter Display: Standard Approvals: UL & C-UL & CE . .",865,"ΤΕΜ",1,"PI1",1,"7ML57442BB000A"]
["7ML5744-2CB00-0A"," SITRANS RD300 Display: remote digital panel mount process display with current or voltage inputs. Two input, multi-line display, totalizer and pump control. Input voltage: 12 ... 36 V DC; 12 ... 24 V AC, 6 W max. Output: 4 Relays Type: Dual input process Meter Display: Standard Approvals: UL & C-UL & CE . .",928,"ΤΕΜ",1,"PI1",1,"7ML57442CB000A"]
["7ML5744-2DB00-0A  "," SITRANS RD300 Display: remote digital panel mount process display with current or voltage inputs. Two input, multi-line display, totalizer and pump control. Input voltage: 12 ... 36 V DC; 12 ... 24 V AC, 6 W max. Output: 4 ... 20 mA output Type: Dual input process Meter Display: Standard Approvals: UL & C-UL & CE . .",896,"ΤΕΜ",1,"PI1",1,"7ML57442DB000A"]
["7ML5744-2EB00-0A  ","SITRANS RD300 Display: remote digital panel mount process display with current or voltage inputs. Two input, multi-line display, totalizer and pump control. Input voltage: 12 ... 36 V DC; 12 ... 24 V AC, 6 W max. Output: 2 Relays and 4 ... 20 mA output Type: Dual input process Meter Display: Standard Approvals: UL & C-UL & CE . . ",956,"ΤΕΜ",1,"PI1",1,"7ML57442EB000A"]
["7ML5744-2FB00-0A  ","SITRANS RD300 Display: remote digital panel mount process display with current or voltage inputs. Two input, multi-line display, totalizer and pump control. Input voltage: 12 ... 36 V DC; 12 ... 24 V AC, 6 W max. Output: 4 Relays and 4 ... 20 mA output Type: Dual input process Meter Display: Standard Approvals: UL & C-UL & CE . . ",1025,"ΤΕΜ",1,"PI1",1,"7ML57442FB000A"]
["7MH4950-1AA01","SIWAREX U WEIGHING ELECTRONICS (SINGLE CHANNEL VERSION) FOR CONNNECTING ONE SCALE FOR SIMATIC S7-300 AND ET200M RS232 INTERFACE FOR CONNECT. OF A PC TTY INTERFACE FOR REMOTE DISPLAY CONNECTION WITH BUS CONNECTOR ",792,"ΤΕΜ",1,"PI3",1,"7MH49501AA01"]
["7MH4950-2AA01","SIWAREX U WEIGHING ELECTRONICS (TWO-CHANNEL VERSION) * FOR CONNNECTING TWO SCALES * FOR SIMATIC S7-300 AND ET200M * RS232 INTERFACE FOR CONNECT. OF A PC * TTY INTERFACE FOR REMOTE DISPLAY CONNECTION WITH BUS CONNECTOR ",1233,"ΤΕΜ",1,"PI3",1,"7MH49502AA01"]
["7MH4910-0AA01","SIWAREX CS WEIGHING ELECTRONIC FOR CONNECTING ONE SCALE. FOR LEGAL TRADE 2000D FOR SIMATIC ET200S-HEAD STATION IM151-1 BASIC/STANDARD/HIGH FEATURE AND IM151-7 CPU. RS232- INTERFACE FOR CONNECTION OF A PC. TTY-INTERFACE FOR REMOTE DISPLAY. ",695,"ΤΕΜ",1,"PI3",1,"7MH49100AA01"]
["7MH4900-2AA01","SIWAREX FTA WEIGHING ELECTRONIC WITH VERIFICATION CAPABILITY.FOR AUTOMATIC AND NON AUTOMATIC . WEIGHING APPLICATIONS. USABLE FOR S7-300 AND ET200M. EC-CERTIFICATE OF CONFORMITY 3 X 6000D. . APPLICATIONS: . RAPID DOSING, FILLING/BAGGING AND LOADING. ATTENTION: FOR LEGAL FOR TRADE APPLICATIONS PLEASE FOLLOW THE LOCAL LAWS APPLYING IN THE COUNTRY OF LEGAL VERIFICATION ! - APPROPRIATE MMC-CARD: ONLY FOR LEGAL-FOR-TRADE APPLICATIONS R76, R51 AND R107: 7MH4900-2AY20 ",1757,"ΤΕΜ",1,"PI3",1,"7MH49002AA01"]
["7MH4900-3AA01","SIWAREX FTC WEIGHING ELECTRONIC FOR FORCE MEASUREMENT, BELT SCALE, LOSS-IN-WEIGHT SCALE AND FLOW RATE METER. WITHOUT VERIFICATION CAPABILITY USABLE FOR S7-300 AND ET200M ",1810,"ΤΕΜ",1,"PI3",1,"7MH49003AA01"]
["7MH4960-2AA01","SIWAREX WP231 calibratable weighing electronic (1 channel) for strain gauge load cells / full bridges (1-4 mV/V) for SIMATIC S7-1200 or stand alone, RS485 and Ethernet-Interface, onboard I/O: 4 DI / 4 DO, 1 AO (0/4...20mA), attention: for calibratable applications please follow the local laws applying in the country of verification! ",546,"ΤΕΜ",1,"PI3",1,"7MH49602AA01"]
["7MH4960-4AA01","SIWAREX WP241 belt weigher electronic (1 channel) for strain gauge load cells / full bridges (1-4mV/V) for SIMATIC S7-1200 or stand alone, RS485 and Ethernet-Interface, onboard I/O: 4 DI / 4 DO 1 AO (0/4...20mA) ",1040,"ΤΕΜ",1,"PI3",1,"7MH49604AA01"]
["7MH4960-6AA01","SIWAREX WP251 calibratable weighing electronic for batching and filling process (1 channel) for strain gauge load cells / full bridges (1-4 mV/V) for SIMATIC S7-1200 or stand alone, RS485 and Ethernet-Interface, onboard I/O: 4 DI / 4 DO, 1 AO (0/4...20mA), attention: for calibratable applications please follow the local laws applying in the country of verification! ",923,"ΤΕΜ",1,"PI3",1,"7MH49606AA01"]
["7MH4138-6AA00-0BA0","SIWAREX WP321 WEIGHING ELECTRONIC (1 CHANNEL) FOR STRAIN GAUGE LOAD CELLS / FULL BRIDGES (1-4 mV/V) FOR SIMATIC ET200SP, FITS to BU-TYPE A0, RS485- INTERFACE FOR CONNECTION OF SIWATOOL OR A REMOTE DISPLAY ",549,"ΤΕΜ",1,"PI3",1,"7MH41386AA000BA0"]
["7MH4980-1AA01","SIWAREX WP521 ST WEIGHING ELECTRONIC (1 CHANNEL) FOR STRAIN GAUGE LOAD CELLS / FULL BRIDGES (1-4 mV/V) FOR SIMATIC S7-1500, RS485 AND ETHERNET-INTERFACE, ONBOARD I/O: DI 3 X 24V DC / DQ 4 X 24V DC ",670,"ΤΕΜ",1,"PI3",1,"7MH49801AA01"]
["7MH4980-2AA01","SIWAREX WP522 ST WEIGHING ELECTRONIC (2 CHANNELS) FOR STRAIN GAUGE LOAD CELLS / FULL BRIDGES (1-4 mV/V) FOR SIMATIC S7-1500, RS485 AND ETHERNET-INTERFACE, ONBOARD I/O PER CHANNEL: DI 3 X 24V DC / DQ 4 X 24V DC ",1124,"ΤΕΜ",1,"PI3",1,"7MH49802AA01"]
["7MH4900-1AK01","Service and commissioning software SIWATOOL V4 and V7 for SIWAREX weighing modules ",242,"ΤΕΜ",1,"PI3",1,"7MH49001AK01"]
["7MH4607-8CA","SIWAREX U CONNECTING CABLE 9-PIN -FOR SERIAL LINKING OF SIWAREX U W.9-PIN PC NTERFACE (RS232C) - CABLE LENGTH 3 M ",48,"ΤΕΜ",1,"PI3",1,"7MH46078CA"]
["7MH4702-8CA","SIWAREX M CONNECTING CABLE 9-PIN -FOR SERIAL LINKING OF SIWAREX M W.9-PIN PC NTERFACE (RS232C) - CABLE LENGTH 2 M ",49,"ΤΕΜ",1,"PI3",1,"7MH47028CA"]
["7MH5001-0AA20","Junction box SIWAREX JB; die-cast aluminum quality to connect in parallel up to 4 load cells in 4-wire or 6-wire system; degree of protection: IP66; dimensions: 100 x 160 x 81 mm ",396,"ΤΕΜ",1,"PI3",1,"7MH50010AA20"]
["7MH5001-0AA00","Junction box SIWAREX JB; stainless steel housing to connect in parallel up to 4 load cells in 4-wire or 6-wire system; degree of protection: IP66; dimensions: 150 x 100 x 61 mm ",501,"ΤΕΜ",1,"PI3",1,"7MH50010AA00"]
["7MH5001-0AD20","SIWAREX DB digital junction box for enhanced diagnostics, 4 channels die-cast aluminum enclosure for connection of strain gauge load cells/full bridges (1-4mV/V) to SIWAREX weighing electronics type of protection: IP66 dimensions: 100 x 160 x 81 mm ",842,"ΤΕΜ",1,"PI3",1,"7MH50010AD20"]
["7MH4710-5BA","SIWAREX IS Ex barrier for intrinsically safe connection of load cells mounting on standard rail, standard version Certified according to ATEX: (EEX IB) II C as associated equipment metrological approval ",1179,"ΤΕΜ",1,"PI3",1,"7MH47105BA"]
["7MH4710-5CA","SIWAREX IS INTERMEDIATE BOX FOR INTRINSIC SAFE CONNECTION OF LOAD CELLS, LOW-CURRENT WITH ATEX APPROVAL: (EEX IB) II C AS ASSOCIATED ELECTRICAL EQUIPMENT ",1351,"ΤΕΜ",1,"PI3",1,"7MH47105CA"]
["7MH4702-8AF","LI2Y 2X0,75ST + 2X (2X0,34ST) -CY SPECIAL CABLE, WITH BLUE SHEATH CONNECTION OF JB JUNCTION AND DISTRIBUTION BOX IN AN AREA SUBJECT TO EXPLOSION HAZARDS AND IB INTERMEDIATE BOX FOR PERMANENT ON-SITE INSTALLATION; OCCASIONAL BENDING POSSIBLE, APPROX. 10.8 MM OUTER DIAMETER, AMBIENT TEMPERATURE -40 TO +80 CEL. CABLE CUT TO LENGTH, WITHOUT CONNECTOR. ",6,"ΤΕΜ",1,"PI3",1,"7MH47028AF"]
["7MH4702-8AG","LI2Y 2X0,75ST + 2 (2X0,34ST) - CY, SHEATH ORANGE, SPECIAL CABLE FOR CONNECTION SIWAREX MODULE TO JB JUNCTION BOX AND DISTRIBUTION BOX OR IB INTER- MEDIATE BOX AS WELL AS BETWEEN TWO IB'S FOR PERMANENT ON-SITE INSTALLATION;OCCASIONAL BENDING POSSIBLE. 10.8 MM OUTER DIAMETER AMBIENT TEMPERATURE -40 TO +80 CEL. ",6,"ΤΕΜ",1,"PI3",1,"7MH47028AG"]
["7MH4965-2AA01","SIWAREX WT231 Weighing Terminal Weighing Terminal for use with Platformscales, Binweighing and further. - Stainless steel enclusure with 9 feed troughs - includes SIWAREX WP231, - SIMATIC KTP400 Basic Color PN - Far range power supply 100-240 VAC - IP65, Temperature range: 0-40 degrees cel. ",1578,"ΤΕΜ",1,"PI3",1,"7MH49652AA01"]
["7MH4965-4AA01","SIWAREX WT241 Weighing Terminal Weighing Terminal for use with Beltscales. - Stainless steel enclusure with 9 feed troughs - includes SIWAREX WP241, - SIMATIC KTP400 Basic Color PN - Far range power supply 100-240 VAC - IP65, Temperature range: 0-40 degrees cel. ",2298,"ΤΕΜ",1,"PI3",1,"7MH49654AA01"]
["7MH5102-1KD00","Siwarex WL 260 Load Cell SP-S AA 3kg C3 - Rated load 3 kg - Accuracy class C3 - 3 m Cable length, 6 Conductor - Material Aluminium - Degree of protection IP65 ",104,"ΤΕΜ",1,"PI1",1,"7MH51021KD00"]
["7MH5102-1PD00","Siwarex WL 260 Load Cell SP-S AA 5kg C3 - Rated Load 5kg - Accuracy class C3 - 3m Cable length, 6 Conductor - Material Aluminium - Degree of protection IP65 ",104,"ΤΕΜ",1,"PI1",1,"7MH51021PD00"]
["7MH5102-2AD00","Siwarex WL 260 Load Cell SP-S AA 10kg C3 - Rated load 10 kg - Accuracy class C3 - 3 m Cable length, 6 Conductor - Material Aluminium - Degree of protection IP65 ",104,"ΤΕΜ",1,"PI1",1,"7MH51022AD00"]
["7MH5102-2GD00","Siwarex WL 260 Load Cell SP-S AA 20kg C3 - Rated Load 20kg - Accuracy class C3 - 3m Cable length, 6 Conductor - Material Aluminium - Degree of protection IP65 ",104,"ΤΕΜ",1,"PI1",1,"7MH51022GD00"]
["7MH5102-2PD00","Siwarex WL 260 Load Cell SP-S AA 50kg C3 - Rated Load 50kg - Accuracy class C3 - 3m Cable length, 6 Conductor - Material Aluminium - Degree of protection IP65 ",104,"ΤΕΜ",1,"PI1",1,"7MH51022PD00"]
["7MH5102-3AD00","Siwarex WL 260 Load Cell SP-S AA 100kg C3 - Rated Load 100kg - Accuracy class C3 - 3m Cable length, 6 Conductor - Material Aluminium - Degree of protection IP65 ",104,"ΤΕΜ",1,"PI1",1,"7MH51023AD00"]
["7MH5104-1PD00","Siwarex WL 260 Load Cell SP-S SA 5kg C3 - Rated Load 5kg - Accuracy class C3 - 1m Cable length, 6 Conductor - Material Stainless steel - Degree of protection IP67 ",529,"ΤΕΜ",1,"PI1",1,"7MH51041PD00"]
["7MH5104-2AD00","Siwarex WL 260 Load Cell SP-S SA 10kg C3 - Rated Load 10kg - Accuracy class C3 - 1m Cable length, 6 Conductor - Material Stainless steel - Degree of protection IP67 ",529,"ΤΕΜ",1,"PI1",1,"7MH51042AD00"]
["7MH5104-2GD00","Siwarex WL 260 Load Cell SP-S SA 20kg C3 - Rated Load 20kg - Accuracy class C3 - 1m Cable length, 6 Conductor - Material Stainless steel - Degree of protection IP67 ",529,"ΤΕΜ",1,"PI1",1,"7MH51042GD00"]
["7MH5104-2PD00","Siwarex WL 260 Load Cell SP-S SA 50kg C3 - Rated Load 50kg - Accuracy class C3 - 1m Cable length, 6 Conductor - Material Stainless steel - Degree of protection IP67 ",529,"ΤΕΜ",1,"PI1",1,"7MH51042PD00"]
["7MH5104-3AD00","Siwarex WL 260 Load Cell SP-S SA 100kg C3 - Rated Load 100kg - Accuracy class C3 - 1m Cable length, 6 Conductor - Material Stainless steel - Degree of protection IP67 ",529,"ΤΕΜ",1,"PI1",1,"7MH51043AD00"]
["7MH5104-3GD00","Siwarex WL 260 Load Cell SP-S SA 200kg C3 - Rated Load 200kg - Accuracy class C3 - 1m Cable length, 6 Conductor - Material Stainless steel - Degree of protection IP67 ",529,"ΤΕΜ",1,"PI1",1,"7MH51043GD00"]
["7MH5106-2AD00","Siwarex WL 230 Load Cell BB-S SA 10kg C3 - Rated Load 10kg - Accuracy class C3 - 3m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP68 ",377,"ΤΕΜ",1,"PI1",1,"7MH51062AD00"]
["7MH5106-2GD00","Siwarex WL 230 Load Cell BB-S SA 20kg C3 - Rated Load 20kg - Accuracy class C3 - 3m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP68 ",377,"ΤΕΜ",1,"PI1",1,"7MH51062GD00"]
["7MH5106-2PD00","Siwarex WL 230 Load Cell BB-S SA 50kg C3 - Rated Load 50kg - Accuracy class C3 - 3m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP68 ",377,"ΤΕΜ",1,"PI1",1,"7MH51062PD00"]
["7MH5106-3AD00","Siwarex WL 230 Load Cell BB-S SA 100kg C3 - Rated Load 100kg - Accuracy class C3 - 3m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP68 ",377,"ΤΕΜ",1,"PI1",1,"7MH51063AD00"]
["7MH5106-3GD00","Siwarex WL 230 Load Cell BB-S SA 200kg C3 - Rated Load 200kg - Accuracy class C3 - 3m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP68 ",377,"ΤΕΜ",1,"PI1",1,"7MH51063GD00"]
["7MH5106-3LD00","Siwarex WL 230 Load Cell BB-S SA 350kg C3 - Rated Load 350kg - Accuracy class C3 - 3m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP68 ",397,"ΤΕΜ",1,"PI1",1,"7MH51063LD00"]
["7MH5106-3PD00","Siwarex WL 230 Load Cell BB-S SA 500kg C3 - Rated Load 500kg - Accuracy class C3 - 3m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP68 ",405,"ΤΕΜ",1,"PI1",1,"7MH51063PD00"]
["7MH5107-3PD00","Siwarex WL 230 Load Cell SB-S SA 500kg C3 - Rated Load 500kg - Accuracy class C3 - 3m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP68 ",389,"ΤΕΜ",1,"PI1",1,"7MH51073PD00"]
["7MH5107-4AD00","Siwarex WL 230 Load Cell SB-S SA 1t C3 - Rated Load 1t - Accuracy class C3 - 3m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP68 ",421,"ΤΕΜ",1,"PI1",1,"7MH51074AD00"]
["7MH5107-4GD00","Siwarex WL 230 Load Cell SB-S SA 2t C3 - Rated Load 2t - Accuracy class C3 - 6m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP68 ",421,"ΤΕΜ",1,"PI1",1,"7MH51074GD00"]
["7MH5107-4PD00","Siwarex WL 230 Load Cell SB-S SA 5t C3 - Rated Load 5t - Accuracy class C3 - 6m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP68 ",460,"ΤΕΜ",1,"PI1",1,"7MH51074PD00"]
["7MH5105-2PD00","Siwarex WL 250 Load Cell ST-S SA 50kg C3 - Rated Load 50kg - Accuracy class C3 - 6m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP67 ",396,"ΤΕΜ",1,"PI1",1,"7MH51052PD00"]
["7MH5105-3AD00","Siwarex WL 250 Load Cell ST-S SA 100kg C3 - Rated Load 100kg - Accuracy class C3 - 6m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP67 ",396,"ΤΕΜ",1,"PI1",1,"7MH51053AD00"]
["7MH5105-3HD00","Siwarex WL 250 Load Cell ST-S SA 250kg C3 - Rated Load 250kg - Accuracy class C3 - 6m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP67 ",396,"ΤΕΜ",1,"PI1",1,"7MH51053HD00"]
["7MH5105-3PD00","Siwarex WL 250 Load Cell ST-S SA 500kg C3 - Rated Load 500kg - Accuracy class C3 - 6m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP67 ",396,"ΤΕΜ",1,"PI1",1,"7MH51053PD00"]
["7MH5105-4AD00","Siwarex WL 250 Load Cell ST-S SA 1t C3 - Rated Load 1t - Accuracy class C3 - 6m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP67 ",421,"ΤΕΜ",1,"PI1",1,"7MH51054AD00"]
["7MH5105-4HD00","Siwarex WL 250 Load Cell ST-S SA 2,5t C3 - Rated Load 2,5t - Accuracy class C3 - 6m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP67 ",529,"ΤΕΜ",1,"PI1",1,"7MH51054HD00"]
["7MH5105-4PD00","Siwarex WL 250 Load Cell ST-S SA 5t C3 - Rated Load 5t - Accuracy class C3 - 6m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP67 ",553,"ΤΕΜ",1,"PI1",1,"7MH51054PD00"]
["7MH5105-5AD00","Siwarex WL 250 Load Cell ST-S SA 10t C3 - Rated Load 10t - Accuracy class C3 - 6m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP67 ",1210,"ΤΕΜ",1,"PI1",1,"7MH51055AD00"]
["7MH5108-3PD00","Load Cell Siwarex WL 270 CP-S SA 0.5t C3, Rated Load 0.5t, Accuracy class C3, not legal for trade, 15m Cable length, 4 Conductor, Material Stainless steel, Type of protection IP68. ",632,"ΤΕΜ",1,"PI1",1,"7MH51083PD00"]
["7MH5108-4AD00","Load cell Siwarex WL 270 CP-S SA 1t C3, Rated load 1 metric ton, Accuracy class C3, Not legal for trade, 15 m connecting cable, 4 conductors, material stainless steel, Enclosure rating IP68, ",632,"ΤΕΜ",1,"PI1",1,"7MH51084AD00"]
["7MH5108-4GD00","Siwarex WL 270 Load Cell CP-S SA 2t C3 - Rated Load 2t - Accuracy acc. to class C3 - without approval - 15m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP68 ",643,"ΤΕΜ",1,"PI1",1,"7MH51084GD00"]
["7MH5108-4PD00","Siwarex WL 270 Load Cell CP-S SA 5t C3 - Rated Load 5t - Accuracy acc. to class C3 - without approval - 15m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP68 ",643,"ΤΕΜ",1,"PI1",1,"7MH51084PD00"]
["7MH5108-5AD00","Siwarex WL 270 Load Cell CP-S SA 10t C3 - Rated Load 10t - Accuracy class C3 - 15m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP68 ",643,"ΤΕΜ",1,"PI1",1,"7MH51085AD00"]
["7MH5108-5GD00","Siwarex WL 270 Load Cell CP-S SA 20t C3 - Rated Load 20t - Accuracy class C3 - 15m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP68 ",643,"ΤΕΜ",1,"PI1",1,"7MH51085GD00"]
["7MH5108-5KD00","Siwarex WL 270 Load Cell CP-S SA 30t C3 - Rated Load 30t - Accuracy class C3 - 15m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP68 ",643,"ΤΕΜ",1,"PI1",1,"7MH51085KD00"]
["7MH5108-5PD00","Siwarex WL 270 Load Cell CP-S SA 50t C3 - Rated Load 50t - Accuracy class C3 - 15m Cable length, 4 Conductor - Material Stainless steel - Degree of protection IP68 ",643,"ΤΕΜ",1,"PI1",1,"7MH51085PD00"]
["7MH5113-2QD00","Siwarex WL 280 Load Cell RN-S SA 60kg C3 - Rated Load 60kg - Accuracy class C3 according to OIML R60, - 3 m Cable length, 4 Wires - Made of Stainless steel - protection class IP68 ",1133,"ΤΕΜ",1,"PI1",1,"7MH51132QD00"]
["7MH5113-3DD00","Siwarex WL 280 Load Cell RN-S SA 130kg C3 - Rated Load 130kg - Accuracy class C3 according to OIML R60, - 3 m Cable length, 4 Wires - Made of Stainless steel - protection class IP68 ",1133,"ΤΕΜ",1,"PI1",1,"7MH51133DD00"]
["7MH5113-3JD00","Siwarex WL 280 Load Cell RN-S SA 280kg C3 - Rated Load 280kg - Accuracy class C3 according to OIML R60, - 3 m Cable length, 4 Wires - Made of Stainless steel - protection class IP68 ",1133,"ΤΕΜ",1,"PI1",1,"7MH51133JD00"]
["7MH5113-3PD00","Siwarex WL 280 Load Cell RN-S SA 500kg C3 - Rated Load 500kg - Accuracy class C3 according to OIML R60, - 3 m Cable length, 4 Wires - Made of Stainless steel - protection class IP68 ",1133,"ΤΕΜ",1,"PI1",1,"7MH51133PD00"]
["7MH5113-4AD00","Siwarex WL 280 Load Cell RN-S SA 1t C3 - Rated Load 1t - Accuracy class C3 according to OIML R60, - 3 m Cable length, 4 Wires - Made of Stainless steel - protection class IP68 ",1133,"ΤΕΜ",1,"PI1",1,"7MH51134AD00"]
["7MH5113-4GD00","Siwarex WL 280 Load Cell RN-S SA 2t C3 - Rated Load 2t - Accuracy class C3 according to OIML R60, - 6 m Cable length, 4 Wires - Made of Stainless steel - protection class IP68 ",1133,"ΤΕΜ",1,"PI1",1,"7MH51134GD00"]
["7MH5113-4LD00","Siwarex WL 280 Load Cell RN-S SA 3,5t C3 - Rated Load 3,5t - Accuracy class C3 according to OIML R60, - 6 m Cable length, 4 Wires - Made of Stainless steel - protection class IP68 ",1133,"ΤΕΜ",1,"PI1",1,"7MH51134LD00"]
["7MH5113-4PD00","Siwarex WL 280 Load Cell RN-S SA 5t C3 - Rated Load 5t - Accuracy class C3 according to OIML R60, - 6 m Cable length, 4 Wires - Made of Stainless steel - protection class IP68 ",1374,"ΤΕΜ",1,"PI1",1,"7MH51134PD00"]
["7MH5113-5AD00","Siwarex WL 280 Load Cell RN-S SA 10t C3 - Rated Load 10t - Accuracy class C3 according o OIML R60, - 15m Cable length, 4 Wires - Made of Stainless steel - protection class IP68 ",1456,"ΤΕΜ",1,"PI1",1,"7MH51135AD00"]
["7MH5113-5DD00","Siwarex WL 280 Load Cell RN-S SA 13t C3 - Rated Load 13t - Accuracy class C3 according o OIML R60, - 15m Cable length, 4 Wires - Made of Stainless steel - protection class IP68 ",1619,"ΤΕΜ",1,"PI1",1,"7MH51135DD00"]
["7MH5113-5JD00","Siwarex WL 280 Load Cell RN-S SA 28t C3 - Rated Load 28t - Accuracy class C3 according o OIML R60, - 15m Cable length, 4 Wires - Made of Stainless steel - protection class IP68 ",1782,"ΤΕΜ",1,"PI1",1,"7MH51135JD00"]
["7MH5113-5QD00","Siwarex WL 280 Load Cell RN-S SA 60t C3 - Rated Load 60t - Accuracy class C3 according o OIML R60, - 15m Cable length, 4 Wires - Made of Stainless steel - protection class IP68 ",2106,"ΤΕΜ",1,"PI1",1,"7MH51135QD00"]

{"sheet":"Sheet1","index":1,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["PA","PMD Data available"]
[""]
["VF","Sales Release"]
[""]
["LF","Delivery Release"]
[""]
["AE","Phase Out Announce"]
[""]
["TS","Prod. Cancellation"]
[""]
["MH","Prod. Discont."]
[""]
["AK","End Prod.Lifecycl."]