{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Price List 2016","Sheet1"],"not_rendered":{"charts":0,"images":3,"macros":1,"external_links":0,"defined_names":3,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Price List 2016","index":0,"n_rows":76296,"n_cols":8,"rows_kept":4500,"cut":true,"hidden":false,"merged":[[1,0,1,7],[2,2,2,7],[0,3,0,7],[0,1,0,2],[2,0,2,1]],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
[null,"Digital Factory / Process Industries and Drives \nΓενικός Τιμοκατάλογος Προϊόντων Βιομηχανίας 2017",null,"Ισχύει μέχρι την 30.09.2017 και καταργεί κάθε προηγούμενο. Οι τιμές και τα τεχνικά χαρακτηριστικά των υλικών υπόκεινται σε οποιαδήποτε αλλαγή χωρίς προηγούμενη ειδοποίηση και δεν περιλαμβάνουν ΦΠΑ. "]
["Περιλαμβάνει τις παρακάτω κατηγορίες υλικών:"]
["Βιομηχανικός αυτοματισμός Simatic και Υλικά Δικτύου (Simatic)\nΒιομηχανικός αυτοματισμός Simatic S71200 (S71200)\nLOGO!, τροφοδοτικά LOGO! Power (LOGO!)\n",null,"Διανομή ισχύος χαμηλής τάσης και Τεχνολογία ηλεκτρικών εγκαταστάσεων (LP) \nΡυθμιστές στροφών και συστήματα ελέγχου κίνησης  Motion control (MC)\nΚινητήρες AC (LD) \nΒιομηχανικό υλικό χαμηλής τάσης (CP)"]
["Αναζήτηση υλικού","Αναζήτηση σε:"]
["Κωδικός","Περιγραφή","Τιμή καταλόγου (€)","Μον. Μέτρησης","Ποσ. μονάδας μέτρησης","Κατηγορία υλικού","Βάρος (KG)","Ελάχιστη ποσότητα παραγγελίας"]
["6DD16000BA3","SIMATIC TDC, CPU551 64-BIT CPU MODULE WITH DIGITAL INPUTS",8021,"TEM",1,"Simatic",0.58099999999999996,1]
["6DD16000BB0","SIMATIC TDC, CPU555 64-BIT CPU MODULE WITH PROFINET IRT",10506,"TEM",1,"Simatic",0.77100000000000002,1]
["6DD16070AA2","SIMATIC S7-400, FM458-1 DP  APPLICATION MODULE FOR SIMATIC S7-400",5286,"TEM",1,"Simatic",1.1619999999999999,1]
["6DD16070CA1","SIMATIC S7-400, EXM 438-1 I/O EXPANSION MODULE FOR FM 458 4 X ANALOG OUTPUTS 16 BIT EXM 438-1 NOT SPAREPART COMPATIBLE TO EXM438",3837,"TEM",1,"Simatic",1.0309999999999999,1]
["6DD16070EA2","SIMATIC S7-400, COMUNICATION EXPANSION MODULE EXM 448-2 WITH 2 SIMOLINK INTERFACES",2508,"TEM",1,"Simatic",0.91700000000000004,1]
["6DD16070GA0","SIMATIC S7-400, FM458-1DP KNOW-HOW-PROTECT",412,"TEM",1,"Simatic",2.5000000000000001E-2,1]
["6DD16100AH3","SIMATIC TDC MEMORY CARD MC521 2 MB FLASH-EPROM, 8 KB EEPROM",608,"TEM",1,"Simatic",4.7E-2,1]
["6DD16100AH4","SIMATIC TDC MEMORYCARD MC500 4MB FLASH-EPROM, 8 KB EEPROM",678,"TEM",1,"Simatic",4.8000000000000001E-2,1]
["6DD16100AH6","SIMATIC TDC MEMORYCARD MC510 8 MB FLASH-EPROM, 8 KB EEPROM EEPROM",977,"TEM",1,"Simatic",4.7E-2,1]
["6DD16400AH0","SIMATIC TDC SIGNALMODULE SM500 WITH 8 AO/8 AI/16 DO/16 DI/ 4 INCREMENTAL ENCODER INPUTS/ 4 ABSOLUTE ENCODER INPUTS/ 6 LED",2988,"TEM",1,"Simatic",0.55800000000000005,1]
["6DD16600BF0","SIMATIC TDC COMMUNICATION MODULE CP52M0 MEMORY MODULE FR GLOBAL DATA MEMORY (GDM) WITH 2 MBYTE SRAM MEMORY",6081,"TEM",1,"Simatic",0.46500000000000002,1]
["6DD16600BG0","SIMATIC TDC COMMUNICATION MODULE CP52IO INTERFACE MODULE FOR GLOBAL DATA MEMORY (GDM) WITH 4 INTERFACES",9353,"TEM",1,"Simatic",0.54200000000000004,1]
["6DD16600BH0","SIMATIC TDC COMMUNICATION MODULE CP52AO ACCESS MODULE FOR GLOBAL DATA MEMORY (GDM)",5661,"TEM",1,"Simatic",0.46800000000000003,1]
["6DD16600BJ0","SIMATIC TDC CP53M0 COMMUNICATION MODULE RACK COUPLING TDC <--> SIMADYN",6598,"TEM",1,"Simatic",0.503,1]
["6DD16610AD1","SIMATIC TDC COMMUNICATION MODULE CP50M1 WITH 8 MBYTE BUFFER MEMORY, UP TO 1 MPI INTERFACE, UP TO 2 PROFIBUS DP INTERFACES",3968,"TEM",1,"Simatic",0.52100000000000002,1]
["6DD16610AE1","SIMATIC TDC COMMUNICATION MODULE CP51M1 FOR INDUSTRIAL ETHERNET WITH TCP/IP AND/OR UDP",3497,"TEM",1,"Simatic",0.5,1]
["6DD16800BB0","SIMATIC TDC, CONNECTOR PLUG SM11 INTERFACE MODULE , 5 PLUGS",108,"TEM",1,"Simatic",1.6E-2,1]
["6DD16810AE2","SIMATIC TDC, BINARY INPUT OR OUTPUT SB10 8 BI OR 8 BO , 24V DC LED DISPLAY",188,"TEM",1,"Simatic",0.378,1]
["6DD16810AF4","SIMADYN D BINARY INPUT MODULE SB60 8 BI, 115V AC/DC, LED-DISPLAY, GALVANIC ISOLATION",508,"TEM",1,"Simatic",0.41299999999999998,1]
["6DD16810AG2","SIMATIC TDC, BINARY OUTPUT MODULE SB70 8 BO, MAX. 120V AC/DC, LED-DISPLAY, GALVANIC ISOLATION",340,"TEM",1,"Simatic",0.46600000000000003,1]
["6DD16810AJ1","SIMATIC TDC, CONVERTER SU12 10-POLE 10 SCREW-PLUGIN-TERMINALS 10-POLE PLUG",207,"TEM",1,"Simatic",0.35499999999999998,1]
["6DD16810DH1","SIMATIC TDC, BINARY OUTPUT MODULE SB71 8 BI, 24 OR 48 V DC LED-DISPLAY, GALVANIC ISOLATION",408,"TEM",1,"Simatic",0.47299999999999998,1]
["6DD16810EB3","SIMATIC TDC, BINARY INPUT MODULE SB61 GALVANIC ISOLATION24/48V , 8BI 24 OR 48 V DC, LED-DISPLAY",496,"TEM",1,"Simatic",0.42599999999999999,1]
["6DD16810GK0","SIMATIC TDC, CONVERTER SU13 50 TERMINALS (1:1 CONNECTION)",205,"TEM",1,"Simatic",0.39,1]
["6DD16820CH3","SIMATIC TDC, SUBRACK UR6021, 21 SLOTS, VMEBUS,  8 P0 SLOTS, EXCHANGEABLE FANS, SUITABLE FOR GDM, 5-ROW FEMALE CONNECTOR",6763,"TEM",1,"Simatic",20.5,1]
["6DD16820DA1","SIMATIC TDC SLOT COVER SR51",73.7,"TEM",1,"Simatic",0.4,1]
["6DD16830CH3","SIMATIC TDC, FAN TRAY FOR SUB RACK UR6021",4227,"TEM",1,"Simatic",3.8,1]
["6DD16840GC0","SIMATIC TDC PLUGIN CABLE SC62, 50-POLE SCREENED, LENGTH: 2M",358,"TEM",1,"Simatic",0.53,1]
["6DD16840GD0","SIMATIC TDC PLUGIN CABLE SC63 50-POLE SCREENED, LENGTH: 2M",240,"TEM",1,"Simatic",0.30299999999999999,1]
["6DD16840GE0","SIMATIC S7-400, PLUGIN CABLE SC64 9/10POLE FOR CONNECTING OF A SBXX/SU12- INTERFACEMODULES TO DIGITAL INPUTS IF FM458; LEGTH: 2M",90.7,"TEM",1,"Simatic",0.14099999999999999,1]
["6DD16840GG0","SIMATIC TDC PLUGIN CABLE SC66 10-POLE SCREENED, LENGTH: 2M",56,"TEM",1,"Simatic",0.13200000000000001,1]
["6DD16840GH0","SIMATIC TDC SERVICE CABLE SC67 TO CONNECT TO THE CPU-SERVICE-INTERFACE 10-POLE SCREENED, LENGTH: 7M",72.5,"TEM",1,"Simatic",0.20599999999999999,1]
["6DD18055DA0","SIMATIC D7-FB GENERATOR V2.1 INCL. SERVICE PACK 2; SINGLE LICENSE F. 1 INSTALL., E-SW, SW AND DOKU ON CD, CLASS A, 2 LANGUAGES (G,E), EXECUTABLE UNDER WIN98SE/ME/ WIN NT/2000/XP, REFERENCE HARDWARE: SIMATIC FM 458, T400, SIMATIC TDC, SIMADYN D",1149,"TEM",1,"Simatic",0.22,0]
["6ED10521CC010BA8","LOGO! 24CE,LOGIC MODULE,DISPLAY PU/I/O: 24V/24V/24V TRANS., 8DI (4AI)/4DO; MEM 400 BLOCKS, EXPANDABLE, ETHERNET BUILD IN WEB-SERVER, DATALOG STANDARD MICRO SD CARD FOR LOGO! SOFT COMFORT V8 PREVIOUS PROJECT USABLE",120,"TEM",1,"LOGO!",0.246,1]
["6ED10521FB000BA8","LOGO!230RCE,LOGIC MODULE,DISPL. PU/I/O: 115V/230V/RELAY, 8 DI/4 DO; MEM 400 BLOCKS EXPANDABLE, ETHERNET BUILD IN WEB-SERVER, DATALOG STANDARD MICRO SD CARD FOR LOGO! SOFT COMFORT V8 PREVIOUS PROJECT USABLE",139,"TEM",1,"LOGO!",0.23899999999999999,1]
["6ED10521HB000BA8","LOGO! 24RCE,LOGICMODULE,DISPLAY PU/I/O: 24V AC/24V DC/RELAY, 8 DI/4 DO; MEM. 400 BLOCKS, EXPANDABLE, ETHERNET BUILD IN WEB-SERVER, DATALOG STANDARD MICRO SD CARD FOR LOGO! SOFT COMFORT V8 PREVIOUS PROJECT USABLE",136,"TEM",1,"LOGO!",0.28999999999999998,1]
["6ED10521MD000BA8","LOGO!12/24RCE,LOGIC MOD.,DISPL. PU/I/O: 12/24V DC/RELAY, 8 DI (4AI)/4 DO; MEM 400 BLOCKS EXPANDABLE, ETHERNET BUILD IN WEB-SERVER, DATALOG STANDARD MICRO SD CARD FOR LOGO! SOFT COMFORT V8 PREVIOUS PROJECT USABLE",136,"TEM",1,"LOGO!",0.29599999999999999,1]
["6ED10522CC010BA8","LOGO! 24CEO, LOGIC MODULE, WITHOUT DISPLAY, PU/I/O: 24V/24V/24V TRANS., 8 DI (4AI)/4 DO; MEM 400 BLOCKS EXPANDABLE, ETHERNET BUILD IN WEB-SERVER, DATALOG STANDARD MICRO SD CARD FOR LOGO! SOFT COMFORT V8 PREVIOUS PROJECT USABLE",104,"TEM",1,"LOGO!",0.21099999999999999,1]
["6ED10522FB000BA8","LOGO! 230RCEO, LOGIC MODULE, PS/I/O: 230V/230V/RELAY, 8DI/4DO; W/O DISPLAY, MEMORY 400 BLOCKS, EXPANDABLE MODULAR, ETHERNET BUILD IN WEB-SERVER, DATALOG STANDARD MICRO SD CARD FOR LOGO! SOFT COMFORT V8 OR HIGHER PREVIOUS PROJECT USABLE",112,"TEM",1,"LOGO!",0.254,1]
["6ED10522HB000BA8","LOGO! 24RCO (AC), LOGIC MODULE, PU/I/O: 24V AC/24V DC/RELAY, 8 DI/4 DO; W/O DISPLAY, MEMORY 400 BLOCKS, EXPANDABLE, ETHERNET BUILD IN WEB-SERVER, DATALOG STANDARD MICRO SD CARD FOR LOGO! SOFT COMFORT V8 PREVIOUS PROJECT USABLE",109,"TEM",1,"LOGO!",0.254,1]
["6ED10522MD000BA8","LOGO! 12/24RCEO, LOGIC MODULE PU/I/O: 12/24V DC/RELAY, 8 DI (4AI)/4 DO; W/O DISPLAY, MEMORY 400 BLOCKS EXPANDABLE, ETHERNET BUILD IN WEB-SERVER, DATALOG STANDARD MICRO SD CARD FOR LOGO! SOFT COMFORT V8 PREVIOUS PROJECT USABLE",109,"TEM",1,"LOGO!",0.25,1]
["6ED10551CB000BA2","LOGO! DM8 24  EXPANSION MODULE, PU/I/O: 24V/24V/TRANS., 4 DI/4 DO FOR LOGO! 8",65.100000000000009,"TEM",1,"LOGO!",0.13600000000000001,1]
["6ED10551CB100BA2","LOGO! DM16 24,  EXP. MODULE PU/I/O: 24V DC/24V DC/TRANS., 8 DI/8 DO, 4TE FOR LOGO! 8",107,"TEM",1,"LOGO!",0.23400000000000001,1]
["6ED10551FB000BA2","LOGO! DM8 230R, EXP. MODULE, PU/I/O: 230V/230V/RELAIS, 2TE, 4 DI/4 DO FOR LOGO! 8",70.400000000000006,"TEM",1,"LOGO!",0.17199999999999999,1]
["6ED10551FB100BA2","LOGO! DM16 230R, EXP. MODULE, PU/I/O: 230V/230V/RELAIS, 4TE, 8 DI/8 DO FOR LOGO! 8",115,"TEM",1,"LOGO!",0.30099999999999999,1]
["6ED10551HB000BA2","LOGO! DM8 24R EXPANSION MODULE, PU/I/O: 24V/24V/RELAY, 2TE 4 DI/4 DO,  AC/DC/NPN INPUT FOR LOGO! 8",70.400000000000006,"TEM",1,"LOGO!",0.17199999999999999,1]
["6ED10551MA000BA2","LOGO! AM2  EXPANSION MODULE, PU: DC 12/24V, 2 AI, 0 - 10V OR 0/4 - 20MA FOR LOGO! 8",86.100000000000009,"TEM",1,"LOGO!",0.13700000000000001,1]
["6ED10551MB000BA2","LOGO! DM8 12/24R, EXP. MODULE PU/I/O: 12, 24V/12V/24V/RELAIS, 2TE, 4 DI/4 DO FOR LOGO! 8",70.400000000000006,"TEM",1,"LOGO!",0.17199999999999999,1]
["6ED10551MD000BA2","LOGO! AM2  RTD EXPAN. MODULE, PU: DC 12/24V, 2AI, -50 ... +200 DEGR/C PT100/1000 FOR LOGO! 8",104,"TEM",1,"LOGO!",0.13600000000000001,1]
["6ED10551MM000BA2","LOGO! AM2 AQ EXPAN. MODULE, PU: DC 24V, 0/4-20MA 2AQ, 0-10V FOR LOGO! 8",123,"TEM",1,"LOGO!",0.13700000000000001,1]
["6ED10551NB100BA2","LOGO! DM16 24R, EXP.  MODULE, PU/I/O: 24V DC/24V DC/RELAY, 8 DI/8 DO, 4TE FOR LOGO! 8",115,"TEM",1,"LOGO!",0.29899999999999999,1]
["6ED10554MH000BA1","LOGO! TD TEXTDISPLAY, 6 LINES, 3 BACKGROUND COLORS 2 ETHERNET PORTS ACCESSORIES, FOR LOGO! 8",154,"TEM",1,"LOGO!",0.32,1]
["6ED10571DA000BA0","LOGO! TD MOUNTING ACCESSORIES, SPARE PARTS FOR LOGO! TD",11.600000000000001,"TEM",1,"LOGO!",3.1E-2,1]
["6ED10573BA000AA8","LOGO! STARTER KIT 12/24RCE WITH LOGO! 12/24RCE, LOGO! SOFT COMFORT V8, WINCC BASIC POWER SUPPLY IN SYSTAINER",285,"TEM",1,"Simatic",2.367,0]
["6ED10573BA020AA8","LOGO! STARTER KIT 230RCE LOGO! 230RCE, LOGO! SOFT COMFORT V8, SCREWDRIVER WINCC BASIC V13 IN SYSTAINER",254,"TEM",1,"Simatic",2.38,0]
["6ED10573BA100AA8","LOGO! TD STARTER KIT 12/24V WITH LOGO! TD, LOGO! 12/24RCEO, LOGO! SOFT COMFORT V8 SCREWDRIVER WINCC BASIC V13 INSYSTAINER POWER SUPPLY",407,"TEM",1,"Simatic",2.82,0]
["6ED10573SA000YA1","LOGO! TRAINING PACK. 24V WITH 5 PIECES  LOGO! 12/24RC, 5 LOGO! SOFT COMFORT, 1 LOGO! PC CABLE, 10 LANGUAGES GE/EN/FR/IT/SP/CN/TR/RUS/JP/NL, EXECUTABLE UNDER WIN98SE/NT4.0/ME/2000/XP/VISTA, MAC OS X, LINUX, REFERENCE-HW: LOGO! FOR EDUCATIONAL PURPOSES ONLY",489,"TEM",1,"Simatic",0.97,0]
["6ED10573SA000YB1","LOGO! TRAINING PACK. 230V WITH 5 PIECES LOGO! 230RC, 5 LOGO! SOFT COMFORT, 1 LOGO! PC CABLE, 10 LANGUAGES GE/EN/FR/IT/SP/CN/TR/RUS/JP/NL, EXECUTABLE UNDER WIN98SE/NT4.0/ME/2000/XP/VISTA, MAC OS X, LINUX, REFERENCE-HW: LOGO! FOR EDUCATIONAL PURPOSES ONLY",489,"TEM",1,"Simatic",0.97,0]
["6ED10573SA000YC0","LOGO! TRAINING PACK. PC CABLE WITH 4 PIECES LOGO! PC CABLE FOR EDUCATIONAL PURPOSES ONLY",244,"TEM",1,"Simatic",0.7,0]
["6ED10573SA200YA1","LOGO! 8 TRAINING PACK. 12/24RCE WITH 6 PIECES  LOGO! 12/24RCE, 6 LOGO! DM8 12/24R, 6 LOGO! SOFT COMFORT, 6 LANGUAGES GE/EN/FR/IT/SP/CN, EXECUTABLE UNDER WINXP (32 BIT), WIN7 (32&64 BIT), WIN8 (32&64 BIT), MAC OS X, LINUX, REFERENCE-HW: LOGO! FOR EDUCATIONAL PURPOSES ONLY",975,"TEM",1,"Simatic",3.6,0]
["6ED10573SA200YB1","LOGO! 8 TRAINING PACKAGE 230RCE WITH 6 PIECES   LOGO! 230RCE, 6 LOGO! DM8 230R, 6 LOGO! SOFT COMFORT, 6 LANGUAGES GE/EN/FR/IT/SP/CN, EXECUTABLE UNDER WINXP (32 BIT), WIN7 (32&64 BIT), WIN8 (32&64 BIT), MAC OS X, LINUX, REFERENCE-HW: LOGO! FOR EDUCATIONAL PURPOSES ONLY",975,"TEM",1,"Simatic",3,0]
["6ED10574CA000AA0","LOGO! CONTACT 24 SWITCHING MODULE FOR DIRECT SWITCHING OF RESISTIVE CONS. UPTO 20A AND MOTORS UPTO 4 KW, 24V DC, 3 NO + 1 NC CONTACTS EAN: 4025515050742",18.900000000000002,"TEM",1,"LOGO!",0.16,0]
["6ED10574EA000AA0","LOGO! CONTACT 230 SWITCHING MODULE FOR DIRECT SWITCHING OF RESISTIVE CONS. UPTO 20A AND MOTORS UPTO 4 KW, 230V AC, 3 NO + 1 NC CONTACTS EAN: 4025515050759",15.8,"TEM",1,"LOGO!",0.157,0]
["6ED10580BA080YA1","LOGO! SOFT COMFORT V8, SINGLE LICENSE, FOR 1 INSTALLATION E-SW,SW AND DOCU. ON DVD, 6-LANGUAGES, EXECUTABLE UNDER WINXP, WIN7, WIN8 ALL VERISONS, 32/64 BIT MAC OSX 10.6 .. 10.9 LINUX SUSE 11.3, SP3, K 3.0.76",52.5,"TEM",1,"LOGO!",9.8000000000000004E-2,0]
["6ED10580CA080YE1","LOGO! SOFT COMFORT V8, UPGRADE F. LSC FROM V8 SINGLE LICENSE, F. 1 INSTALLAT. E-SW, SW AND DOCU ON DVD 6-LANGUAGES, EXECUTABLE UNDER WINXP, WIN7, WIN8 ALL VERISONS, 32/64 BIT MAC OSX 10.6 .. 10.9 LINUX SUSE 11.3, SP3, K 3.0.76",20.5,"TEM",1,"LOGO!",9.8000000000000004E-2,0]
["6ES54974UC11","SIMATIC, EXTRACTION TOOL FOR CRIMP CONTACTS",13.200000000000001,"TEM",1,"Simatic",0.2,1]
["6ES57108MA11","SIMATIC,STAND.SECTIONAL RAIL WIDTH 35MM, LENGTH 483MM FOR 19 IN.CABINETS",28.400000000000002,"TEM",1,"Simatic",0.44,0]
["6ES57108MA21","SIMATIC,STAND.SECTIONAL RAIL WIDTH 35MM, LENGTH 530MM FOR 600MM CABINETS",34.4,"TEM",1,"Simatic",0.46600000000000003,0]
["6ES57108MA31","SIMATIC,STAND.SECTIONAL RAIL WIDTH 35MM, LENGTH 830MM FOR 900MM CABINETS",50,"TEM",1,"Simatic",0.82,0]
["6ES57108MA41","SIMATIC,STAND.SECTIONAL RAIL WIDTH 35MM, LENGTH 2M",79.600000000000009,"TEM",1,"Simatic",1.93,0]
["6ES57288MA11","SIMATIC, GROUND TERMINAL 10 PIECES PER PACKAGING UNIT",50.900000000000006,"ΠΑΚ",1,"Simatic",0.311,0]
["6ES71314BB010AA0","SIMATIC DP, 5 ELECTRON. MODULES FOR ET 200S, 2 DI STANDARD 24V DC, 15 MM WIDTH, 5 PIECES PER PACKAGING UNIT",76.600000000000009,"ΠΑΚ",1,"Simatic",0.17100000000000001,1]
["6ES71314BB010AB0","SIMATIC DP, 5 ELECTRON. MODULES FOR ET 200S, 2 DI HIGH FEATURE 24V DC, 15 MM WIDTH WITH PARAM. F. INPUT DELAY DIAGNOSIS F. ENCODER SHORT- CIRCUIT W. LED SF (GROUP FAULT) 5 PIECES PER PACKAGING UNIT",111,"ΠΑΚ",1,"Simatic",0.17499999999999999,1]
["6ES71314BD010AA0","SIMATIC DP, 5 ELECTRON. MODULES FOR ET 200S, 4 DI STANDARD 24V DC, 15 MM WIDTH, 5 PIECES PER PACKAGING UNIT",126,"ΠΑΚ",1,"Simatic",0.17399999999999999,1]
["6ES71314BD010AB0","SIMATIC DP, 5 ELECTRON. MODULES FOR ET 200S, 4 DI HIGH FEATURE 24V DC, 15 MM WIDTH WITH PARAM. F. INPUT DELAY DIAGNOSIS F. ENCODER SHORT- CIRCUIT W. LED SF (GROUP FAULT) 5 PIECES PER PACKAGING UNIT",174,"ΠΑΚ",1,"Simatic",0.17699999999999999,1]
["6ES71314BF000AA0","SIMATIC DP, 1 ELECTR. MODULE FOR ET 200S, 8 DI DC 24V 15 MM WIDTH, 1 PIECE PER PACKAGING UNIT",43.2,"TEM",1,"Simatic",4.2000000000000003E-2,1]
["6ES71314BF004AA0","SIMATIC DP, 100 ELECTR. MODULES FOR ET 200S, 8 DI DC 24V, 15 MM WIDTH, 100 PIECES PER PACKAGING UNIT",4305,"ΠΑΚ",1,"Simatic",3.69,0]
["6ES71314BF500AA0","SIMATIC DP, 1 ELECTRON. MODULE FOR ET 200S, 8 DI SOURCE INPUT 24V DC, 15 MM WIDTH, 1 PIECE PER PACKAGING UNIT",43.2,"TEM",1,"Simatic",4.1000000000000002E-2,1]
["6ES71314CD020AB0","SIMATIC DP, 5 ELECTRON. MODULES ET 200S: 4DI UC 24V...48V, 15 MM WIDTH, WITH LED SF (GROUP FAULT), 5 PIECES PER PACKAGING UNIT",201,"ΠΑΚ",1,"Simatic",0.19900000000000001,1]
["6ES71314EB000AB0","SIMATIC DP, 5 ELECTRON. MODULES FOR ET 200S, 2 DI 120V AC 15 MM WIDTH 5 PIECES PER PACKAGING UNIT",176,"ΠΑΚ",1,"Simatic",0.16900000000000001,1]
["6ES71314FB000AB0","SIMATIC DP, 5 ELECTRON. MODULES FOR ET 200S, 2 DI 230V AC 15 MM WIDTH 5 PIECES PER PACKAGING UNIT",176,"ΠΑΚ",1,"Simatic",0.17100000000000001,1]
["6ES71314RD020AB0","SIMATIC DP, 1 ELECTRON. MODULE ET 200S: 4DI DC 24V NAMUR, 15 MM WIDTH, WITH LED SF (GROUP FAULT),",130,"TEM",1,"Simatic",4.4999999999999998E-2,1]
["6ES71316BF000AA0","SIMATIC ET 200SP, DIGITAL INPUT MODULE, DI 8X24VDC BASIC, PACKING UNIT: 1 PIECE, FITS TO BU-TYPE A0, COLOR CODE CC01, MODULE DIAGNOSIS",44.300000000000004,"TEM",1,"Simatic",0.04,1]
["6ES71316BF000BA0","SIMATIC ET 200SP, DIGITAL INPUT MODULE, DI 8X 24VDC STANDARD, FITS TO BU-TYPE A0, COLOR CODE CC01, MODULE DIAGNOSIS",46.7,"TEM",1,"Simatic",3.6999999999999998E-2,1]
["6ES71316BF000CA0","SIMATIC ET 200SP, DIGITAL INPUT MODULE, DI 8X 24VDC HIGH FEATURE FITS TO BU-TYPE A0, COLOR CODE CC01, CHANNEL DIAGNOSIS",53.800000000000004,"TEM",1,"Simatic",3.6999999999999998E-2,1]
["6ES71316BF000DA0","SIMATIC ET 200SP, DIGITAL INPUT MODULE, DI 8X24VDC HIGH SPEED, PACKING UNIT: 1 PIECE, THREE ALTERNATIVE MODES: DI, OVERSAMPLING, 4 X COUNTER, FITS TO BU-TYPE A0, COLOR CODE CC01",103,"TEM",1,"Simatic",0.04,1]
["6ES71316BF002AA0","SIMATIC ET 200SP, DIGITAL INPUT MODULE, DI 8X24VDC BASIC, PACKING UNIT: 10 PIECES, FITS TO BU-TYPE A0, COLOR CODE CC01, MODULE DIAGNOSIS",44.300000000000004,"TEM",1,"Simatic",0.4,0]
["6ES71316BF002BA0","SIMATIC ET 200SP, DIGITAL INPUT MODULE, DI 8X 24VDC STANDARD, PACKING UNIT: 10 PIECES, FITS TO BU-TYPE A0, COLOR CODE CC01, MODULE DIAGNOSIS",46.7,"TEM",1,"Simatic",0.4,0]
["6ES71316BF600AA0","SIMATIC ET 200SP, DIGITAL INPUT MODULE, DI 8X 24VDC SOURCE INPUT BA, FITS TO BU-TYPE A0, COLOR CODE CC02,",47.2,"TEM",1,"Simatic",3.5000000000000003E-2,1]
["6ES71316BH000BA0","SIMATIC ET 200SP, DIGITAL INPUT MODULE, DI 16X 24VDC STANDARD, FITS TO BU-TYPE A0, COLOR CODE CC00, MODULE DIAGNOSIS",79.800000000000011,"TEM",1,"Simatic",3.6999999999999998E-2,1]
["6ES71316BH002BA0","SIMATIC ET 200SP, DIGITAL INPUT MODULE, DI 16X 24VDC STANDARD, PACKING UNIT: 10 PIECES, FITS TO BU-TYPE A0, COLOR CODE CC00, MODULE DIAGNOSIS",79.800000000000011,"TEM",1,"Simatic",0.4,0]
["6ES71316FD000BB1","SIMATIC ET 200SP, DIGITAL INPUT MODULE, DI 4X120..230VAC STANDARD FITS TO BU-TYPE B1, COLOR CODE CC41, MODULE DIAGNOSIS",57.800000000000004,"TEM",1,"Simatic",4.5999999999999999E-2,1]
["6ES71316TF000CA0","SIMATIC ET 200SP, DIGITAL INPUT MODULE, DI 8X NAMUR HIGH FEATURE, FITS TO BU-TYPE A0, COLOR CODE CC01, CHANNEL DIAGNOSIS",229,"TEM",1,"Simatic",0.04,1]
["6ES71324BB010AA0","SIMATIC DP, 5 ELECTRON. MODULES FOR ET 200S, 2 DO STANDARD DC 24V/0.5A, 15 MM WIDTH 5 PIECES PER PACKAGING UNIT",108,"ΠΑΚ",1,"Simatic",0.17599999999999999,1]
["6ES71324BB010AB0","SIMATIC DP, 5 ELECTRON. MODULES FOR ET 200S, 2 DO HIGH FEATURE 24V DC, 15 MM WIDTH DIAGNOSIS F. SHORT-CIRCUIT AND OPEN-CIRCUIT, FIRST-UP SIGNAL WITH LED SF (GROUP FAULT), 5 PIECES PER PACKAGING UNIT",149,"ΠΑΚ",1,"Simatic",0.185,1]
["6ES71324BB310AA0","SIMATIC DP, 5 ELECTRON. MODULES FOR ET 200S, 2 DO STANDARD DC 24V/2A, 15 MM WIDTH 5 PIECES PER PACKAGING UNIT",195,"ΠΑΚ",1,"Simatic",0.17699999999999999,1]
["6ES71324BB310AB0","SIMATIC DP, 5 ELECTRON. MODULES FOR ET 200S, 2 DO HIGH FEATURE DC 24V/2A, 15 MM WIDTH DIAGNOSIS F. SHORT-CIRCUIT AND OPEN-CIRCUIT, FIRST-UP SIGNAL WITH LED SF (GROUP FAULT), 5 PIECES PER PACKAGING UNIT",236,"ΠΑΚ",1,"Simatic",0.19800000000000001,1]
["6ES71324BD000AB0","SIMATIC DP, 5 ELECTRON. MODULES FOR ET 200S, 4 DO HIGH FEATURE DC 24V/0.5A, 15 MM WIDTH DIAGNOSIS SHORT CIRCUIT, SF-LED 5 PIECES PER PACKAGING UNIT",195,"ΠΑΚ",1,"Simatic",0.17699999999999999,1]
["6ES71324BD020AA0","SIMATIC DP, 5 ELECTRON. MODULES FOR ET 200S, 4 DO STANDARD DC 24V/0.5A, 15 MM WIDTH, 5 PIECES PER PACKAGING UNIT",172,"ΠΑΚ",1,"Simatic",0.17699999999999999,1]
["6ES71324BD300AB0","SIMATIC DP, 5 ELECTRON. MODULES FOR ET 200S, 4 DO SHIGH FEATURE 24V/2A DC, 15 MM WIDTH DIAGNOSIS SHORT CIRCUIT, SF-LED 5 PIECES PER PACKAGING UNIT",350,"ΠΑΚ",1,"Simatic",0.19,1]
["6ES71324BD320AA0","SIMATIC DP, 5 ELECTRON. MODULES FOR ET 200S, 4 DO STANDARD DC 24V/2A, 15 MM WIDTH 5 PIECES PER PACKAGING UNIT",331,"ΠΑΚ",1,"Simatic",0.184,1]
["6ES71324BF000AA0","SIMATIC DP, 1 ELECTRON. MODULE FOR ET 200S, 8 DO DC24V/0,5A, 15 MM WIDTH, 1 PIECE PER PACKAGING UNIT",49.900000000000006,"TEM",1,"Simatic",4.2999999999999997E-2,1]
["6ES71324BF000AB0","SIMATIC DP, 1 ELECTRON. MODULE FOR ET 200S, 8 DO HIGH FEATURE DC24V/0,5A, 15 MM WIDTH, DIAGNOSIS SHORT CIRCUIT, SF-LED 1 PIECES PER PACKAGING UNIT",53.900000000000006,"TEM",1,"Simatic",4.2999999999999997E-2,1]
["6ES71324BF004AA0","SIMATIC DP, 100 ELECTR. MODULES FOR ET 200S, 8 DO DC24V/0,5A, 15 MM WIDTH, 100 PIECES PER PACKAGING UNIT",4982,"ΠΑΚ",1,"Simatic",3.9529999999999998,0]
["6ES71324BF500AA0","SIMATIC DP, 1 ELECTRON. MODULES FOR ET 200S, 8 DO SINK OUTPUT, DC24V/0,5A, 15 MM WIDTH, 1 PIECES PER PACKAGING UNIT",49.900000000000006,"TEM",1,"Simatic",4.2000000000000003E-2,1]
["6ES71324FB010AB0","SIMATIC DP, 5 ELECTRON. MODULES FOR ET 200S, 2 DO 24...230V AC, 15 MM WIDTH 5 PIECES PER PACKAGING UNIT",314,"ΠΑΚ",1,"Simatic",0.19600000000000001,1]
["6ES71324HB010AB0","SIMATIC DP, 5 ELECTRON. MODULES FOR ET 200S, 2 DO RELAY 24V DC - 230V AC/5A,15 MM WIDTH FIRST-UP SIGNAL WITH LED SF (GROUP FAULT), 5 PIECES PER PACKAGING UNIT",172,"ΠΑΚ",1,"Simatic",0.19800000000000001,1]
["6ES71324HB120AB0","SIMATIC DP, 5 ELECTRON. MODULES ET200S: 2DO RELAY(FORM C CONT.) DC24V-48V/5A, AC24V-230V/5A, 15 MM WIDTH, FIRST-UP SIGNAL, 5 PIECES PER PACKAGING UNIT",227,"ΠΑΚ",1,"Simatic",0.23100000000000001,1]
["6ES71324HB500AB0","SIMATIC DP, ELECTRON. MODULE ET200S: 2DO RELAY(FORM C CONT.) DC24V-48V/5A, AC24V-230V/5A, 15 MM WIDTH, FIRST-UP SIGNAL, WITH MANUAL ACTUATION",50.6,"TEM",1,"Simatic",5.3999999999999999E-2,1]
["6ES71326BD200BA0","SIMATIC ET 200SP, DIGITAL OUTPUT MODULE, DQ 4X24VDC/2A STANDARD, FITS TO BU-TYPE A0, COLOR CODE CC02, MODULE DIAGNOSIS",65.400000000000006,"TEM",1,"Simatic",3.6999999999999998E-2,1]
["6ES71326BD200CA0","SIMATIC ET 200SP, DIGITAL OUTPUT MODULE, DQ 4X24VDC/2A HIGH FEATURE, FITS TO BU-TYPE A0, COLOR CODE CC02, CHANNEL DIAGNOSIS",74.600000000000009,"TEM",1,"Simatic",3.6999999999999998E-2,1]
["6ES71326BD200DA0","SIMATIC ET 200SP, DIGITAL OUTPUT MODULE, DQ 4X24VDC/2A HIGH SPEED, PACKING UNIT: 1 PIECE, FITS TO BU-TYPE A0, COLOR CODE CC00; THREE ALTERNATIVE MODES: DQ,OVERSAMPLING, PWM MODULE DIAGNOSIS",156,"TEM",1,"Simatic",0.04,1]
["6ES71326BD202BA0","SIMATIC ET 200SP, DIGITAL OUTPUT MODULE, DQ 4X24VDC/2A STANDARD, PACKING UNIT: 10 PIECES, FITS TO BU-TYPE A0, COLOR CODE CC02, MODULE DIAGNOSIS",65.400000000000006,"TEM",1,"Simatic",0.4,0]
["6ES71326BF000AA0","SIMATIC ET 200SP, DIGITAL OUTPUT MODULE, DQ 8X24VDC/0,5A BASIC, PACKING UNIT: 1 PIECE, FITS TO BU-TYPE A0, COLOR CODE CC02,",58.1,"TEM",1,"Simatic",3.5999999999999997E-2,1]
["6ES71326BF000BA0","SIMATIC ET 200SP, DIGITAL OUTPUT MODULE, DQ 8X24VDC/0,5A STANDARD, FITS TO BU-TYPE A0, COLOR CODE CC02, MODULE DIAGNOSIS",60.400000000000006,"TEM",1,"Simatic",3.5999999999999997E-2,1]
["6ES71326BF000CA0","SIMATIC ET 200SP, DIGITAL OUTPUT MODULE, DQ 8X24VDC/0,5A HIGH FEATURE FITS TO BU-TYPE A0, COLOR CODE CC02, CHANNEL DIAGNOSIS",67.7,"TEM",1,"Simatic",3.5999999999999997E-2,1]
["6ES71326BF002AA0","SIMATIC ET 200SP, DIGITAL OUTPUT MODULE, DQ 8X24VDC/0,5A BASIC, PACKING UNIT: 10 PIECES, FITS TO BU-TYPE A0, COLOR CODE CC02,",58.1,"TEM",1,"Simatic",0.4,0]
["6ES71326BF002BA0","SIMATIC ET 200SP, DIGITAL OUTPUT MODULE, DQ 8X24VDC/0,5A STANDARD, PACKING UNIT: 10 PIECES, FITS TO BU-TYPE A0, COLOR CODE CC02, MODULE DIAGNOSIS",60.400000000000006,"TEM",1,"Simatic",0.4,0]
["6ES71326BF600AA0","SIMATIC ET 200SP, DIGITAL OUTPUT MODULE, DQ 8X24VDC/0,5A SINK BASIC, FITS TO BU-TYPE A0, COLOR CODE CC01",63.800000000000004,"TEM",1,"Simatic",3.6999999999999998E-2,1]
["6ES71326BH000BA0","SIMATIC ET 200SP, DIGITAL OUTPUT MODULE, DQ 16X24VDC/0.5A STANDARD, FITS TO BU-TYPE A0, COLOR CODE CC00, MODULE DIAGNOSIS",92.7,"TEM",1,"Simatic",3.6999999999999998E-2,1]
["6ES71326BH002BA0","SIMATIC ET 200SP, DIGITAL OUTPUT MODULE, DQ 16X24VDC/0.5A STANDARD, PACKING UNIT: 10 PIECES, FITS TO BU-TYPE A0, COLOR CODE CC00, MODULE DIAGNOSIS",92.7,"TEM",1,"Simatic",0.4,0]
["6ES71326FD000BB1","SIMATIC ET 200SP, DIGITAL OUTPUT MODULE, DQ 4X24..230VAC/2A STANDARD FITS TO BU-TYPE B1, COLOR CODE CC41, MODULE DIAGNOSIS",101,"TEM",1,"Simatic",5.8999999999999997E-2,1]
["6ES71326FD002BB1","SIMATIC ET 200SP, DIGITAL OUTPUT MODULE, DQ 4X24..230VAC/2A STANDARD PACKING UNIT: 10 PIECES, FITS TO BU-TYPE B1, COLOR CODE CC41, MODULE DIAGNOSIS",101,"TEM",1,"Simatic",0.59,0]
["6ES71326GD500BA0","SIMATIC ET 200SP, SIGNAL RELAY CHANGE OVER, RQ 4X24VDC/2A CO ST, FITS TO BU-TYPE A0, COLOR CODE CC00, MODULE DIAGNOSIS",46.1,"TEM",1,"Simatic",3.6999999999999998E-2,1]
["6ES71326HD000BB1","SIMATIC ET 200SP, RELAY MODULE NORMALLY OPEN, RQ 4X120VDC..230VAC/5A STANDARD FITS TO BU-TYPE B0 OR B1, MODULE DIAGNOSIS",63,"TEM",1,"Simatic",4.4999999999999998E-2,1]
["6ES71326HD002BB1","SIMATIC ET 200SP, RELAY MODULE NORMALLY OPEN, RQ 4X120VDC..230VAC/5A STANDARD PACKING UNIT: 10 PIECES, FITS TO BU-TYPE B0 OR B1, MODULE DIAGNOSIS",63,"TEM",1,"Simatic",0.4,0]
["6ES71326MD000BB1","SIMATIC ET 200SP, RELAY MODULE NORMALLY OPEN, RQ NO-MA4X120VDC..230VAC/5A ST, WITH MANUAL ACTUATION, PACKAGING UNIT PU 1 FITS TO BU-TYPE B0 OR B1, MODULE DIAGNOSIS",118,"TEM",1,"Simatic",3.5999999999999997E-2,1]
["6ES71336CV151AM0","SIMATIC ET 200SP, 5 BU-COVER, 15MM, TO PROTECT EMPTY SLOTS",21.5,"ΠΑΚ",1,"Simatic",4.7E-2,0]
["6ES71336CV201AM0","SIMATIC ET 200SP, 5 BU-COVER, 20MM, TO PROTECT EMPTY SLOTS",21.5,"ΠΑΚ",1,"Simatic",5.7000000000000002E-2,0]
["6ES71344FB010AB0","SIMATIC DP, ELECTRONIC MODULE FOR ET 200S, 2 AI STANDARD 15 MM WIDE +/-10 V; 13 BIT + SIGN +/-5 V; 12 BIT+ SIGN, 1..5V; 12BIT, CYCLE TIME 65 MS/CHANNEL WITH LED SF (GROUP FAULT)",130,"TEM",1,"Simatic",4.3999999999999997E-2,1]
["6ES71344FB520AB0","SIMATIC DP, ELECTRONIC MODULE ET 200S: 2 AI HIGH SPEED U, 15 BIT, 15 MM WIDE, CYCLE TIME OF MODULE: 0.1MS, WITH LED SF (GROUP FAULT)",285,"TEM",1,"Simatic",5.6000000000000001E-2,1]
["6ES71344GB010AB0","SIMATIC DP, ELECTRONIC MODULE FOR ET 200S, 2 AI STAND. I-2DMU 15 MM WIDE, 4 .. 20MA; 13 BIT FOR 2-WIRE TRANSDUCER CYCLE TIME 65 MS/CHANNEL WITH LED SF (GROUP FAULT)",130,"TEM",1,"Simatic",4.2999999999999997E-2,1]
["6ES71344GB110AB0","SIMATIC DP, ELECTRONIC MODULE FOR ET 200S, 2 AI STAND. I-4DMU 15 MM WIDE, +/-20MA; 13 BIT + SIGN,4 .. 20MA; 12 BIT FOR 4-WIRE TRANSDUCER CYCLE TIME 65 MS/CHANNEL WITH LED SF (GROUP FAULT)",130,"TEM",1,"Simatic",4.2999999999999997E-2,1]
["6ES71344GB520AB0","SIMATIC DP, ELECTRONIC MODULE ET200S: 2AI HIGH SPEED I-2WIRE, 0 - 20MA, 4 - 20MA, 15BIT, 15 MM WIDTH, FOR 2-WIRE TRANSDUCER, CYCLE TIME OF THE MOD.: 0.1MS, WITH LED SF (GROUP FAULT)",285,"TEM",1,"Simatic",5.6000000000000001E-2,1]
["6ES71344GB620AB0","SIMATIC DP, ELECTRONIC MODULE ET 200S: 2AI HIGH SPEED I-4WIRE 4 - 20MA; 16BIT, 15 MM WIDTH, FOR 4-WIRE TRANSDUCER, CYCLE TIME OF MODULE: 0.1MS, WITH LED SF (GROUP FAULT)",285,"TEM",1,"Simatic",5.5E-2,1]
["6ES71344GD000AB0","SIMATIC DP, ELECTRONIC MODULE ET200S, 4AI STANDARD I-2-WIRE, 4 - 20MA; 13BIT, 15MM WIDTH, FOR 2-WIRE TRANSDUCER CYCLE TIME 40 MS/MODULE WITH LED SF (GROUP FAULT)",162,"TEM",1,"Simatic",4.3999999999999997E-2,1]
["6ES71344JB510AB0","SIMATIC DP, ELECTRONIC MODULE FOR ET 200S, 2/4 AI RTD STANDARD, 15 MM WIDE, 15BIT + SIGN PT100 STD; PT100 KL; NI100 STD; NI100 KL; 150 OHM; 300 OHM; 600 OHM, CYCLE TIME 110 MS/CHANNEL WITH LED SF (GROUP FAULT)",185,"TEM",1,"Simatic",4.2999999999999997E-2,1]
["6ES71344JD000AB0","SIMATIC DP, ELECTRONIC MODULE FOR ET 200S, 4 AI TC, +/-80MV; 15 MM WIDE, 15 BIT + SIGN WITH LED SF (GROUP FAULT).",214,"TEM",1,"Simatic",4.3999999999999997E-2,1]
["6ES71344LB020AB0","SIMATIC DP, ELECTRONIC MODULE 2 AI U HIGH FEATURE FOR ET 200S, 15 MM WIDE, CYCLE TIME PER MODULE: 0.5MS, +/-10V; 15 BI + SIGN, +/-5V;15BIT+SIGN, 1..5V; 15BIT, OPERATIONAL LIMITS +/-0.1% WITH LED SF (GROUP FAULT)",172,"TEM",1,"Simatic",5.5E-2,1]
["6ES71344MB020AB0","SIMATIC DP, ELECTRONIC MODULE 2 AI I HIGH FEATURE FOR ET 200S, 15 MM WIDE, CYCLE TIME PER MODULE: 0.5MS, +/-20MA; 15 BIT + SIGN, 4 .. 20MA; 15 BIT, OPERATIONAL LIMITS +/-0.1% WITH LED SF (GROUP FAULT)",172,"TEM",1,"Simatic",4.4999999999999998E-2,1]
["6ES71344NB010AB0","SIMATIC DP, ELECTRONIC MODULE F. ET200S, 2 AI TC HIGH FEATURE 15 MM WIDE, 15 BIT + SIGN WITH INTERNAL STERATURE COMPENSATION",162,"TEM",1,"Simatic",4.4999999999999998E-2,1]
["6ES71344NB510AB0","SIMATIC DP, ELECTRONIC MODULE ET 200S: 2AI RTD HIGH FEATURE, 15 MM WIDTH, 15BIT + SIGN ACCURACY +/- 0.1%, FOR 2-/3-/-4- WIRE SENSORS, WITH INTERNAL COMPENSATION OF THE WIRE RESISTOR, WITH LED SF (GROUP FAULT)",185,"TEM",1,"Simatic",4.2999999999999997E-2,1]
["6ES71346FB000BA1","SIMATIC ET 200SP, ANALOG INPUT MODULE, AI 2XU STANDARD PACKING UNIT: 1 PIECE, FITS TO BU-TYPE A0, A1, COLOR CODE CC00, MODULE DIAGNOSIS, 16BIT",135,"TEM",1,"Simatic",3.9E-2,1]
["6ES71346FF000AA1","SIMATIC ET 200SP, ANALOG INPUT MODULE, AI 8XU BASIC, FITS TO BU-TYPE A0, A1, COLOR CODE CC02, MODULE DIAGNOSIS, 16BIT",213,"TEM",1,"Simatic",3.9E-2,1]
["6ES71346GB000BA1","SIMATIC ET 200SP, ANALOG INPUT MODULE, AI 2XI 2-/4-WIRE STANDARD, PACKING UNIT: 1 PIECE, FITS TO BU-TYPE A0, A1, COLOR CODE CC05, MODULE DIAGNOSIS, 16 BIT",135,"TEM",1,"Simatic",0.04,1]
["6ES71346GD000BA1","SIMATIC ET 200SP, ANALOG INPUT MODULE, AI 4XI 2-/4-WIRE STANDARD, FITS TO BU-TYPE A0, A1, COLOR CODE CC03, MODULE DIAGNOSIS, 16BIT, +/-0,3%",161,"TEM",1,"Simatic",0.04,1]
["6ES71346GF000AA1","SIMATIC ET 200SP, ANALOG INPUT MODULE, AI 8XI 2-/4-WIRE BASIC, FITS TO BU-TYPE A0, A1, COLOR CODE CC01, MODULE DIAGNOSIS, 16BIT",213,"TEM",1,"Simatic",3.6999999999999998E-2,1]
["6ES71346HB000CA1","SIMATIC ET 200SP, ANALOG INPUT MODULE, AI 2X U/I 2-,4-WIRE HIGH FEAT., FITS TO BU-TYPE A0, A1, COLOR CODE CC05, CHANNEL DIAGNOSIS, 16BIT, +/-0,1%",211,"TEM",1,"Simatic",4.1000000000000002E-2,1]
["6ES71346HB000DA1","SIMATIC ET 200SP, ANALOG INPUT MODULE, AI 2 X U/I 2-,4-WIRE HIGH SPEED FITS TO BU-TYPE A0, A1, COLOR CODE CC00, CHANNEL DIAGNOSIS, 16BIT, +/-0,3%",259,"TEM",1,"Simatic",0.04,1]
["6ES71346HD000BA1","SIMATIC ET 200SP, ANALOG INPUT MODULE, AI 4XU/I 2-WIRE STANDARD, FITS TO BU-TYPE A0, A1, COLOR CODE CC03, MODULE DIAGNOSIS, 16BIT, +/-0,3%",161,"TEM",1,"Simatic",3.9E-2,1]
["6ES71346HD002BA1","SIMATIC ET 200SP, ANALOG INPUT MODULE, AI 4XU/I 2-WIRE STANDARD, PACKING UNIT: 10 PIECES, FITS TO BU-TYPE A0, A1, COLOR CODE CC03, MODULE DIAGNOSIS, 16BIT, +/-0,3%",161,"TEM",1,"Simatic",0.4,0]
["6ES71346JD000CA1","SIMATIC ET 200SP, ANALOG INPUT MODULE, AI 4XRTD/TC HIGH FEATURE, FITS TO BU-TYPE A0, A1, COLOR CODE CC00, CHANNEL DIAGNOSIS, 16BIT, +/-0,1%, 2-/3-/4-WIRE",204,"TEM",1,"Simatic",3.9E-2,1]
["6ES71346JD002CA1","SIMATIC ET 200SP, ANALOG INPUT MODULE, AI 4XRTD/TC HIGH FEATURE, PACKING UNIT: 10 PIECES, FITS TO BU-TYPE A0, A1, COLOR CODE CC00, CHANNEL DIAGNOSIS, 16BIT, +/-0,1%, 2-/3-/4-WIRE",204,"TEM",1,"Simatic",3.9E-2,0]
["6ES71346JF000CA1","SIMATIC ET 200SP, ANALOG INPUT MODULE, AI 8XRTD/TC 2-WIRE HIGH FEATURE FITS TO BU-TYPE A0, A1, COLOR CODE CC00, CHANNEL DIAGNOSIS, 16BIT, +/-0,1%",304,"TEM",1,"Simatic",3.9E-2,1]
["6ES71346JF002CA1","SIMATIC ET 200SP, ANALOG INPUT MODULE, AI 8XRTD/TC 2-WIRE HIGH FEATURE PACKING UNIT: 10 PIECES, FITS TO BU-TYPE A0, A1, COLOR CODE CC00, CHANNEL DIAGNOSIS, 16BIT, +/-0,1%",304,"TEM",1,"Simatic",0.4,0]
["6ES71346PA000BD0","SIMATIC ET 200SP, ANALOG INPUT MODULE, AI ENERGY METER ST, FITS TO BU-TYPE D0, CHANNEL DIAGNOSIS,",176,"TEM",1,"Simatic",5.3999999999999999E-2,1]
["6ES71346PA010BD0","SIMATIC ET 200SP, ANALOG INPUT MODULE, AI ENERGY METER 400V AC ST, FITS TO BU-TYPE D0, CHANNEL DIAGNOSIS",176,"TEM",1,"Simatic",5.3999999999999999E-2,1]
["6ES71346PA200BD0","SIMATIC ET 200SP, ANALOG INPUT MODULE, AI ENERGY METER 480VAC ST, FITS TO BU-TYPE D0, CHANNEL DIAGNOSIS",214,"TEM",1,"Simatic",5.3999999999999999E-2,1]
["6ES71354FB010AB0","SIMATIC DP, ELECTRONIC MODULE FOR ET 200S, 2 AO U, 15 MM WIDTH, +/-10 V; 13 BIT + SIGN, 1..5V; 12BIT, CYCLE TIME < 1 MS WITH LED SF (GROUP FAULT)",128,"TEM",1,"Simatic",4.4999999999999998E-2,1]
["6ES71354FB520AB0","SIMATIC DP, ELECTRONIC MODULE FOR ET200S, 2 AO U HIGH SPEED, 15 MM WIDTH, +/-10V, +/-5V, 1.. 5V; 16BIT, CYCLE TIME: 0.1 MS WITH LED SF (GROUP FAULT)",285,"TEM",1,"Simatic",5.6000000000000001E-2,1]
["6ES71354GB010AB0","SIMATIC DP, ELECTRONIC MODULE FOR ET 200S, 2 AO I 15 MM WIDE, +/-20 MA; 13 BIT + SIGN, 4 . .20 MA; 13 BIT CYCLE TIME < 1 MS WITH LED SF (GROUP FAULT)",128,"TEM",1,"Simatic",4.3999999999999997E-2,1]
["6ES71354GB520AB0","SIMATIC DP, ELECTRONIC MODULE FOR ET 200S, 2 AO I HIGH SPEED 15 MM WIDE, +/-20 MA; 16 BIT, 4 . .20 MA; 16 BIT CYCLE TIME 0.1 MS WITH LED SF (GROUP FAULT)",285,"TEM",1,"Simatic",5.5E-2,1]
["6ES71354LB020AB0","SIMATIC DP, ELECTRONIC MODULE 2 AO U HIGH FEATURE FOR ET 200S, 15 MM WIDE, CYCLE TIME PER MODULE: 0.5MS, +/-10V; 15 BIT + SIGN, 1 .. 5V; 15 BIT, OPERATIONAL LIMITS +/-0.07% WITH LED SF (GROUP FAULT)",172,"TEM",1,"Simatic",4.4999999999999998E-2,1]
["6ES71354MB020AB0","SIMATIC DP, ELECTRONIC MODULE 2 AO I HIGH FEATURE FOR ET 200S, 15 MM WIDE, CYCLE TIME PER MODULE: 0.5MS, +/-20MA; 15 BIT + SIGN, 4 .. 20MA; 15 BIT, OPERATIONAL LIMITS +/-0.05% WITH LED SF (GROUP FAULT)",172,"TEM",1,"Simatic",4.4999999999999998E-2,1]
["6ES71356FB000BA1","SIMATIC ET 200SP, ANALOG OUTPUT MODULE, AQ 2XU STANDARD, PACKING UNIT: 1 PIECE, FITS TO BU-TYPE A0, A1, COLOR CODE CC00, MODULE DIAGNOSIS, 16 BIT",152,"TEM",1,"Simatic",3.9E-2,1]
["6ES71356GB000BA1","SIMATIC ET 200SP, ANALOG OUTPUT MODULE, AQ 2XI STANDARD, PACKING UNIT: 1 PIECE, FITS TO BU-TYPE A0, A1, COLOR CODE CC00, MODULE DIAGNOSIS, 16 BIT",152,"TEM",1,"Simatic",3.9E-2,1]
["6ES71356HB000CA1","SIMATIC ET 200SP, ANALOG OUTPUT MODULE, AQ 2XU/I HIGH FEATURE, FITS TO BU-TYPE A0, A1, COLOR CODE CC00, CHANNEL DIAGNOSIS, 16BIT, +/-0,1%",211,"TEM",1,"Simatic",3.9E-2,1]
["6ES71356HB000DA1","SIMATIC ET 200SP, ANALOG OUTPUT MODULE, AQ 2 X U/I HIGH SPEED, FITS TO BU-TYPE A0, A1, COLOR CODE CC00, CHANNEL DIAGNOSIS, 16BIT, +/-0,3%",259,"TEM",1,"Simatic",3.7999999999999999E-2,1]
["6ES71356HD000BA1","SIMATIC ET 200SP, ANALOG OUTPUT MODULE, AQ 4XU/I STANDARD, FITS TO BU-TYPE A0, A1, COLOR CODE CC00, MODULE DIAGNOSIS, 16BIT, +/-0,3%",204,"TEM",1,"Simatic",0.04,1]
["6ES71366BA000AB1","TRAINING BUNDLE SAFETY FOR SIMATIC ET 200SP  CONSISTING OF: 1X F-DI 8X24VDC HF, 1X F-DQ 4X24VDC/2A PM HF, 1X F-RQ DC24V/AC24..230V/5A, 3X BASEUNITS, LABELING STRIPS ******************************* FOR EDUCATIONAL PURPOSES ONLY",698,"TEM",1,"Simatic",0.7,0]
["6ES71366BA000CA0","SIMATIC DP,  ELECTRON. MODULE F. ET 200SP, F-DI 8X24VDC HF, 15 MM WIDTH, UP TO PL E (ISO 13849-1)/ SIL3 (IEC 61508)",202,"TEM",1,"Simatic",0.09,1]
["6ES71366DB000CA0","SIMATIC DP,  ELECTRON. MODULE F. ET 200SP, F-DQ 4XDC 24V/2A, 15 MM WIDTH, UP TO PL E (ISO 13849) UP TO SIL 3 (IEC 61508)",234,"TEM",1,"Simatic",6.8000000000000005E-2,1]
["6ES71366PA000BC0","SIMATIC DP, POWER M. F-PM-E PPM PROFISAFE, FOR ET 200SP; 24V DC FAIL-SAFE SWITCHING OF DQ AND F-DQ UP TO PL D / SIL2 OR PL E / SIL3 2 FAIL-SAFE DIGITAL INPUTS 1 FAIL-SAFE DIGITAL OUTPUT PPM",266,"TEM",1,"Simatic",8.1000000000000003E-2,1]
["6ES71366RA000BF0","SIMATIC DP,  ELECTRON. MODULE FOR ET200SP, F-RQ 1X24VDC/24..230VAC/5A ST, 20MM WIDTH, 1 RELAY OUTPUT (2 NO-CONTACTS) TOTAL OUTPUT CURRENT 5A, RATED VOLTAGE DC 24V AND AC 24 .. 230V, USEABLE UP TO PL E (ISO13849-1: 2008)/ SIL 3 (IEC61508: 2010) IF CONTROLLED BY A F-DQ (E.G. 6ES7136-6DB00-0CA0)",103,"TEM",1,"Simatic",7.1999999999999995E-2,1]
["6ES71376AA000BA0","ET 200SP, CM PTP CM PTP COMMUNICATION MODUL FOR SERIAL CONNECTION RS422, RS485 AND RS232, FREEPORT, 3964(R), USS, MODBUS RTU MASTER, SLAVE, 115200 KBIT/S",289,"TEM",1,"Simatic",0.04,1]
["6ES71376BD000BA0","SIMATIC ET 200SP, CM 4 X IO-LINK ST COMMUNICATION MODULE IO-LINK MASTER V1.1",210,"TEM",1,"Simatic",3.7999999999999999E-2,1]
["6ES71384AA010AA0","SIMATIC DP, 5 RESERVE MODULES FOR ET 200S, 15 MM WIDTH, FOR SLOT RESERVATION OF UNUSED SLOTS, 5 PIECES PER PACKAGING UNIT",68.900000000000006,"ΠΑΚ",1,"Simatic",0.13200000000000001,1]
["6ES71384AA110AA0","SIMATIC DP, 1 RESERVE MODULE FOR ET 200S, 30 MM WIDTH, FOR SLOT RESERVATION OF UNUSED SLOTS,",18.400000000000002,"TEM",1,"Simatic",4.1000000000000002E-2,1]
["6ES71384CA010AA0","SIMATIC DP, POWER MODULE PM-E FOR ET 200S; 24V DC WITH DIAGNOSIS",13.4,"TEM",1,"Simatic",0.04,1]
["6ES71384CA011AA0","SIMATIC DP,5 POWER MODULES PM-E FOR ET 200S; 24V DC WITH DIAGNOSIS 5 PIECES PER PACKAGING UNIT.",66.7,"ΠΑΚ",1,"Simatic",0.17299999999999999,1]
["6ES71384CA500AB0","SIMATIC DP, POWER MODULE PM-E FOR ET 200S; 24V-48V DC WITH DIAGNOSIS",32.800000000000004,"TEM",1,"Simatic",0.04,1]
["6ES71384CA501AB0","SIMATIC DP,5 POWER MODULES PM-E FOR ET 200S; 24V-48V DC WITH DIAGNOSIS 5 PIECES PER PACKAGING UNIT",164,"ΠΑΚ",1,"Simatic",0.18099999999999999,1]
["6ES71384CA600AB0","SIMATIC DP, POWER MODULE PM-E HIGH FEATURE FOR ET 200S; 24V DC WITH DIAGNOSIS",40.200000000000003,"TEM",1,"Simatic",0.04,1]
["6ES71384CA800AB0","SIMATIC DP,POWER MODULE PM-E RO FOR ET 200S; DC 24V WITH DIAGNOSIS",55.2,"TEM",1,"Simatic",4.5999999999999999E-2,1]
["6ES71384CB110AB0","SIMATIC DP, POWER MODULE PM-E FOR ET200S, DC24-48V, AC24-230V, WITH DIAGNOSTICS AND BACKUP",35,"TEM",1,"Simatic",4.2000000000000003E-2,1]
["6ES71384CF030AB0","SIMATIC DP, POWER MODULE PM-E F PROFISAFE, FOR ET 200S; 24V DC USEABLE FOR INSTALLATIONS WITH UNGROUNDED REFERENCE POTENTIAL RELAIS FOR FAIL-SAFE SWITCHING OF VOLTAGE BUSES P1 AND P2 UP TO CATEGORY 3 (EN954-1)/ SIL2 (IEC61508)/PLD (ISO13849), 2 FAIL-SAFE DIGITAL OUTPUTS UP TO CATEGORY 4 (EN954-1)/ SIL3 (IEC61508)/PLE (ISO13849), ALSO USEABLE IN PROFINET-NETWORKS W. IM151-3 HF",320,"TEM",1,"Simatic",0.10199999999999999,1]
["6ES71384CF420AB0","SIMATIC DP, POWER MODULE PM-E F PROFISAFE, FOR ET 200S; 24V DC USEABLE FOR INSTALLATIONS WITH GROUNDED REFERENCE POTENTIAL RELAIS FOR FAIL-SAFE SWITCHING OF VOLTAGE BUS P2 UP TO CATEGORY 3 (EN954-1)/ SIL2 (IEC61508)/PLD (ISO13849), ALSO USEABLE IN PROFINET- NETWORKS WITH IM151-3 HF",320,"TEM",1,"Simatic",9.6000000000000002E-2,1]
["6ES71384DA040AB0","SIMATIC DP, ELECTRONIC MODULE F. ET 200S, 1 COUNT 24V/100KHZ 15 MM WIDE, OPERATION MODES: COUNT, MEASURE, (PERIOD DURATION MEASUREMENT HIGH RESOLUTION) WITH CLOCK CYCLIC SYNCHRON.APP",201,"TEM",1,"Simatic",4.7E-2,1]
["6ES71384DB030AB0","SIMATIC DP, ELECTRONIC MODULE F. ET 200S, 1 SSI 25BIT/1MHZ 15MM WIDE MODULE FOR CONN. OF ABSOLUTE ENCODERS WITH SSI INTERFACE SYNCHRONOUS SERIAL INTERFACE WITH DI AND COMPAR. VALUE WITH CLOCK CYCLIC SYNCHRON. APP",206,"TEM",1,"Simatic",4.5999999999999999E-2,1]
["6ES71384DC010AB0","SIMATIC DP, ELECTRONIC MODULE FOR ET 200S, 1 STEP 5V/204KHZ FOR POSITIONING STEPPER MOTOR 15MM WIDE, SINGLE CHANNEL, +/-5V INTERF. FOR POWER SECTION",323,"TEM",1,"Simatic",4.7E-2,1]
["6ES71384DD010AB0","SIMATIC DP, ELECTRONIC MODULE FOR ET 200S, 2 PULSE PULSED GENERATOR AND TIMER MODULE, 15 MM WIDE, 2 CHANNELS",300,"TEM",1,"Simatic",4.4999999999999998E-2,1]
["6ES71384DE020AB0","SIMATIC DP, ELECTRONIC MODULE FOR ET 200S, 1 COUNT 5V/500KHZ FOR CONNECTING RS442 INCREMENTAL ENCODERS, OPERATION MODES: MEASURE, COUNT 30MM WIDE, SINGLE CHANNEL WITH CLOCK CYCLIC SYNCHRON.APP",264,"TEM",1,"Simatic",7.4999999999999997E-2,1]
["6ES71384DF010AB0","SIMATIC DP, ELECTRONIC MODULE FOR ET 200S, 1 SI SERIAL INTERFACE ONE CHANNEL, 15MM WIDE RS232/422, 485 ASCII, 3964R",293,"TEM",1,"Simatic",4.4999999999999998E-2,1]
["6ES71384DF110AB0","SIMATIC DP, ELECTRONIC MODULE FOR ET 200S, 1 SI SERIAL INTERFACE ONE CHANNEL, 15MM WIDE RS232/422, 485 MODBUS/USS",351,"TEM",1,"Simatic",4.4999999999999998E-2,1]
["6ES71384DL000AB0","SIMATIC DP, ELECTRONIC MODULE FOR ET 200S, 1 POS U, CONTROLLED  POSITIONING WITH DIGITAL OUTPUTS FOR 5V/24V INCREMENTAL ENCODER, SSI-ENCODER, 30MM WIDE",323,"TEM",1,"Simatic",7.8E-2,1]
["6ES71384FA050AB0","SIMATIC DP,  ELECTRON. MODULE F. ET200S, 4/8 F-DI PROFISAFE, 24V DC, 30 MM WIDTH UP TO PL E (ISO13849), UP TO SIL3 (IEC 61508), ALSO USEABLE IN PROFINET- NETWORK WITH IM151-3 HF",217,"TEM",1,"Simatic",8.5999999999999993E-2,1]
["6ES71384FB040AB0","SIMATIC DP,  ELECTRON. MODULE F. ET200S, 4 F-DO PROFISAFE, DC 24V/2A, 30 MM WIDTH UP TO PL E (ISO13849), UP TO SIL 3 (IEC 61508), ALSO USEABLE IN PROFINET- NETWORKS WITH IM151-3 HF",251,"TEM",1,"Simatic",9.0999999999999998E-2,1]
["6ES71384FC010AB0","SIMATIC DP,  ELECTRON. MODULE F. ET200S, 4 F-DI/3 F-DO DC24V/2A PROFISAFE, 30 MM WIDTH UP TO CATEGORY 3 (EN954-1)/ SIL2 (IEC61508)/PLD (ISO13849), ALSO USEABLE IN PROFINET- NETWORK WITH IM151-3 HF",357,"TEM",1,"Simatic",8.6999999999999994E-2,1]
["6ES71384FD000AA0","SIMATIC-DP, 4POTDIS F0R ET 200S POTENTIAL DISTRIBUTION MODULE, 15MM WIDTH",19.600000000000001,"TEM",1,"Simatic",3.9E-2,1]
["6ES71384FR000AA0","SIMATIC DP,  ELECTRON. MODULE 1F-RO DC24V/AC24..230V/5A, F. ET200S, 30 MM WIDTH, 1 RELAY OUTPUT (2 NO-CONTACTS) OUTPUT CURRENT 5A, RATED VOLTAGE 24V DC AND 24 ... 230V AC, USEABLE UP TO CATEGORY 4 (EN954-1)/ SIL3 (IEC61508)/PLE (ISO13849), IF CONTROLLED BY A F-DO (E.G. 6ES7138-4FB02-0AB0)",108,"TEM",1,"Simatic",0.109,1]
["6ES71384FS014AB1","TRAINING BUNDLE FAILSAFE ET200S CONTAINS 1 X EM138 4/8 F-DI 24V 1 X EM138 4 F-DO 24V/2A 1 X EM138 1 F-RO, 3 X TM-E30S44-01 ******************************* FOR EDUCATIONAL PURPOSES ONLY ******************************* OPTION TO 6ES7151-3BA20-4AB1 AND 6ES7151-8FB00-4AB1 OFFER LIMITED UNTIL 12-31-2015",570,"TEM",1,"Simatic",0.7,0]
["6ES71384GA500AB0","SIMATIC DP, ELEKTRONIC MODULE FOR ET 200S, 4SI IO-LINK, 4 POINT TO POINT INTERFACES, 15MM WIDE, IO-LINK MASTER",277,"TEM",1,"Simatic",5.5E-2,1]
["6ES71384HA000AB0","SIMATIC DP, DP MASTER INTERFACE FOR IM 151-7 CPU OR IM 151-8 PN/DP (ET200S), MODULE WITH PROFIBUS DP INTERF. (9 PIN SUB-D, FEMALE) AS DP MASTER",462,"TEM",1,"Simatic",0.122,1]
["6ES71386AA000BA0","SIMATIC ET 200SP, TM COUNT 1X24V COUNTING MODULE, 1 CHANNEL FOR 24V INCREMENTAL ENCODER OR 24V PULSES, 3DI, 2DQ",188,"TEM",1,"Simatic",5.2999999999999999E-2,1]
["6ES71386BA000BA0","SIMATIC ET 200SP, TM POSINPUT 1 COUNTING AND POSITON DETECTION MODULE, FOR RS422 INCREMENTAL ENCODER OR SSI ABSOLUTE ENCODER, 2 DI, 2 DQ",215,"TEM",1,"Simatic",5.3999999999999999E-2,1]
["6ES71386CG000BA0","SIMATIC ET 200SP, TM TIMER DIDQ 10X24V TIME BASED DIGITAL INPUTS AND OUTPUTS 4DI, 6DQ WITH TIMESTAMP COUNT, PWM, OVERSAMPLING",268,"TEM",1,"Simatic",5.1999999999999998E-2,1]
["6ES71386DB000BB1","SIMATIC ET 200SP, TM PULSE 2X24V PWM AND PULSE OUTPUT 2 CHANNELS 2 A FOR VALVES AND DC MOTORS",317,"TEM",1,"Simatic",5.2999999999999999E-2,1]
["6ES71414BF000AA0","SIMATIC DP, ELECTRONIC MODULE FOR ET200PRO 8 DI  DC 24V, MODULE DIAGNOSTICS; INCLUSIVE BUS MODULE CONNECTING MODULE IO 6ES7194-4..00-0AA0 MUST BE ORDERED SEPERATELY",75,"TEM",1,"Simatic",0.17499999999999999,1]
["6ES71414BF000AB0","SIMATIC DP, ELECTRONIC MODULES FOR ET200PRO 8 DI  DC 24V HIGH FEATURE, CHANNEL DIAGNOSTICS; SHORT CIRCUIT AND WIRE BREAK; INCLUSIVE BUS MODULE CONNECTING MODULE IO 6ES7194-4..00-0AA0 MUST BE ORDERED SEPERATELY",129,"TEM",1,"Simatic",0.184,1]
["6ES71414BH000AA0","SIMATIC DP, ELECTRONIC MODULE FOR ET200PRO 16 DI DC 24V, MODULE DIAGNOSTICS; INCLUSIVE BUS MODULE CONNECTING MODULE IO 6ES7194-4CB50-0AA0 MUST BE ORDERED SEPERATELY",108,"TEM",1,"Simatic",0.17699999999999999,1]
["6ES71415AF000BA0","SIMATIC ET 200AL, DI 8X24VDC, 4XM12, DEGREE OF PROTECTION IP67",116,"TEM",1,"Simatic",0.1,1]
["6ES71415AH000BA0","SIMATIC ET 200AL, DI 16X24VDC, 8XM12, DEGREE OF PROTECTION IP67",189,"TEM",1,"Simatic",0.1,1]
["6ES71415BF000BA0","SIMATIC ET 200AL, DI 8X24VDC, 8XM8, DEGREE OF PROTECTION IP67",116,"TEM",1,"Simatic",0.17100000000000001,1]
["6ES71416BF000AB0","SIMATIC DP, ET 200ECO PN, 8 DI 24V DC; 4 X M12, DOUBLE-ASSIGNEMENT, DEGREE OF PROTECTION IP67;",242,"TEM",1,"Simatic",0.63400000000000001,1]
["6ES71416BG000AB0","SIMATIC DP, ET 200ECO PN, 8 DI 24V DC; 8 X M12, DEGREE OF PROTECTION IP67",300,"TEM",1,"Simatic",0.96899999999999997,1]
["6ES71416BH000AB0","SIMATIC DP, ET 200ECO PN, 16 DI 24V DC; 8 X M12, DOUBLE-ASSIGNEMENT; DEGREE OF PROTECTION IP67",336,"TEM",1,"Simatic",0.98099999999999998,1]
["6ES71424BD000AA0","SIMATIC DP, ELECTRONIC MODULE FOR ET200PRO, 4 DO DC 24V, 2.0A; MODULE DIAGNOSTICS; INCLUSIVE BUS MODULE, CONNECTING MODULE IO 6ES7194-4..00-0AA0 MUST BE ORDERED SEPERATELY",75,"TEM",1,"Simatic",0.17399999999999999,1]
["6ES71424BD000AB0","SIMATIC DP, ELECTRONIC MODULES FOR ET200PRO 4 DO DC 24V, 2.0A HIGH FEATURE, CHANNEL DIAGNOSTICS; SHORT CIRCUIT AND WIRE BREAK; INCLUSIVE BUS MODULE CONNECTING MODULE IO 6ES7194-4..00-0AA0 MUST BE ORDERED SEPERATELY",113,"TEM",1,"Simatic",0.183,1]
["6ES71424BF000AA0","SIMATIC DP, ELECTRONIC MODULES FOR ET200PRO 8 DO DC 24V, 0.5A MODULE DIAGNOSTICS; INCLUSIVE BUS MODULE, CONNECTING MODULE IO 6ES7194-4..00-0AA0 MUST BE ORDERED SEPERATELY",96.4,"TEM",1,"Simatic",0.17899999999999999,1]
["6ES71425AF000BA0","SIMATIC ET 200AL, DQ 8X24VDC/2A, 8XM12, DEGREE OF PROTECTION IP67",168,"TEM",1,"Simatic",0.1,1]
["6ES71426BF000AB0","SIMATIC DP, ET 200ECO PN, 8 DO DC 24V/1,3A; 4 X M12, DOUBLE-ASSIGNEMENT, DEGREE OF PROTECTION IP67;",279,"TEM",1,"Simatic",0.63700000000000001,1]
["6ES71426BF500AB0","SIMATIC DP, ET 200ECO PN, 8 DO 24V DC/0,5A; 4 X M12, DOUBLE-ASSIGNEMENT, 1 LOAD VOLTAGE SUPPLY DO DEGREE OF PROTECTION IP67",263,"TEM",1,"Simatic",0.63400000000000001,1]
["6ES71426BG000AB0","SIMATIC DP, ET 200ECO PN, 8 DO 24V DC/1,3A; 8 X M12, DEGREE OF PROTECTION IP67",335,"TEM",1,"Simatic",0.98099999999999998,1]
["6ES71426BH000AB0","SIMATIC DP, ET 200ECO PN, 16 DO 24V DC/1,3A; 8 X M12, DOUBLE-ASSIGNEMENT DEGREE OF PROTECTION IP67",389,"TEM",1,"Simatic",0.98399999999999999,1]
["6ES71426BR000AB0","SIMATIC DP, ET 200ECO PN, 8 DO 24V DC/2A; 8 X M12, DEGREE OF PROTECTION IP67",436,"TEM",1,"Simatic",0.98,1]
["6ES71434BF000AA0","SIMATIC DP, ELECTRONIC MODULES FOR ET200PRO 4 DIO / 4 DO DC 24V, 0.5A MODULE DIAGNOSTICS; INCLUSIVE BUS MODULE, CONNECTING MODULE IO 6ES7194-4CB50-0AA0 MUST BE ORDERED SEPERATELY",129,"TEM",1,"Simatic",0.17699999999999999,1]
["6ES71434BF500AA0","SIMATIC DP, ELECTRONIC MODULES FOR ET200PRO 4 DI / 4 DO DC 24V, 0.5A MODULE DIAGNOSTICS; INCLUSIVE BUS MODULE, CONNECTING MODULE IO  6ES7194-4..00-0AA0  MUST BE ORDERED SEPERATELY",85.7,"TEM",1,"Simatic",0.17799999999999999,1]
["6ES71435AF000BA0","SIMATIC ET 200AL, DIQ 4+DQ 4X24VDC/0,5A, 4XM12, DEGREE OF PROTECTION IP67",126,"TEM",1,"Simatic",0.1,1]
["6ES71435BF000BA0","SIMATIC ET 200AL, DIQ 4+DQ 4X24VDC/0,5A, 8XM8, DEGREE OF PROTECTION IP67",126,"TEM",1,"Simatic",0.17399999999999999,1]
["6ES71444FF010AB0","SIMATIC DP, ELECTRONIC MODULE FOR ET200PRO 4 AI U HIGH FEATURE, +-10V; 0...10V; +-5V; 1...5V; CHANNEL DIAGNOSTICS; INCLUSIVE BUS MODULE CONNECTING MODULE IO 6ES7194-4..00-0AA0 MUST BE ORDERED SEPERATELY",236,"TEM",1,"Simatic",0.182,1]
["6ES71444GF010AB0","SIMATIC DP, ELECTRONIC MODULE FOR ET200PRO 4 AI I HIGH FEATURE, +-20MA; 0...20MA; 4-20MA CHANNEL DIAGNOSTICS; INCLUSIVE BUS MODULE CONNECTING MODULE IO 6ES7194-4..00-0AA0 MUST BE ORDERED SEPERATELY",236,"TEM",1,"Simatic",0.18099999999999999,1]
["6ES71444JF000AB0","SIMATIC DP, ELECTRONIC MODULES FOR ET200PRO 4 AI RTD HIGH FEATURE, PT100; PT200; PT500; PT1000; NI100; NI200; NI500; NI1000; CHANNEL DIANOSTICS; INCLUSIVE BUS MODULE, CONNECTING MODULE IO 6ES7194-4..00-0AA0 MUST BE ORDERED SEPERATELY",247,"TEM",1,"Simatic",0.18,1]
["6ES71444PF000AB0","SIMATIC DP, ELEKTRONIC MODULE FOR ET200PRO, 4 AI TC HIGH FEATURE, TC TYP B, E, J, K, L, N, R, S,T VOLTAGE +/- 80MV CHANNEL DIANOSTICS; INCL. BUS MODULE, CONNECTING MODULE IO 6ES7194-4..00-0AA0 MUST BE ORDERED SEPERATELY",429,"TEM",1,"Simatic",0.183,1]
["6ES71445KD000BA0","SIMATIC ET 200AL, AI 4XU/I/RTD, 4XM12, DEGREE OF PROTECTION IP67",263,"TEM",1,"Simatic",0.19400000000000001,1]
["6ES71446KD000AB0","SIMATIC DP, ET 200ECO PN, 8 AI (4 U/I + 4 RTD/TC); 8XM12, DEGREE OF PROTECTION IP67",462,"TEM",1,"Simatic",0.97899999999999998,1]
["6ES71446KD500AB0","SIMATIC DP, ET 200ECO PN, 8 AI RTD/TC; 8XM12, DEGREE OF PROTECTION IP67",483,"TEM",1,"Simatic",0.97399999999999998,1]
["6ES71454FF000AB0","SIMATIC DP, ELECTRONIC MODULES FOR ET200PRO 4 AO U HIGH FEATURE, +-10V; 0...10V; 1...5V, CHANNEL DIAGNOSTICS; INCLUSIVE BUS MODULE CONNECTING MODULE IO 6ES7194-4..00-0AA0 MUST BE ORDERED SEPERATELY",258,"TEM",1,"Simatic",0.184,1]
["6ES71454GF000AB0","SIMATIC DP, ELECTRONIC MODULES FOR ET200PRO 4 AO I HIGH FEATURE, +-20MA; 0...20MA; 4-20MA; CHANNEL DIAGNOSTICS; INCLUSIVE BUS MODULE CONNECTING MODULE IO 6ES7194-4..00-0AA0 MUST BE ORDERED SEPERATELY",258,"TEM",1,"Simatic",0.186,1]
["6ES71456HD000AB0","SIMATIC DP, ET 200ECO PN, 4 AO U/I; 4 X M12, DEGREE OF PROTECTION IP67",494,"TEM",1,"Simatic",0.998,1]
["6ES71474JD000AB0","SIMATIC DP, electronic module for ET 200pro 4 IO-Link High-feature, channel diagnoSTics, inclusive bus module, connecting module IO 6ES7194-4CA20-0AA0 muST be ordered separately",258,"TEM",1,"Simatic",0.17,1]
["6ES71475JD000BA0","SIMATIC ET 200AL, CM 4X IO-LINK, 4XM12, DEGREE OF PROTECTION IP67",284,"TEM",1,"Simatic",0.19800000000000001,1]
["6ES71476BG000AB0","SIMATIC DP, ET 200ECO PN, 8 DIO 24V DC/1,3A; 8 X M12, DEGREE OF PROTECTION IP67",375,"TEM",1,"Simatic",0.98,1]
["6ES71484CA000AA0","SIMATIC DP, POWER MODULES FOR ELECTRONIC MODULES  ET 200PRO PM-E, DC 24V INCLUSIVE BUS MODULE CONNECTING MODULE PM-E 6ES7194-4B.00-0AA0 MUST BE ORDERED SEPERATELY",59,"TEM",1,"Simatic",0.17,1]
["6ES71484CA600AA0","SIMATIC DP, POWER MODULES OUTPUT FOR ELECTRONIC MODULES  ET 200PRO PM-O, DC 2X24V INCLUSIVE BUS MODULE CONNECTING MODULE PM-O 6ES7194-4BH00-0AA0 MUST BE ORDERED SEPERATELY",118,"TEM",1,"Simatic",0.183,1]
["6ES71484EA000AA0","SIMATIC DP, PNEUMATIC INTERFACE FOR ET 200PRO 16 DO PNEUMATIC FOR COUPLING WITH FESTO VALVE BLOCK CPV-10 INCLUSIVE BUS MODULE",240,"TEM",1,"Simatic",0.47599999999999998,1]
["6ES71484EB000AA0","SIMATIC DP, PNEUMATIC INTERFACE FOR ET 200PRO 16 DO PNEUMATIC FOR COUPLING WITH FESTO VALVE BLOCK CPV-14 INCLUSIVE BUS MODULE",240,"TEM",1,"Simatic",0.63,1]
["6ES71484FA000AB0","SIMATIC DP,  ET 200PRO FAILSAFE ELECTRONIC MODULE 8/16 F-DI DC24V PROFISAFE, 90 MM WIDTH, UP TO CATEGORY 4 (EN954-1)/ SIL3 (IEC61508)/PLE (ISO13849),",459,"TEM",1,"Simatic",0.311,1]
["6ES71484FC000AB0","SIMATIC DP,  ET 200PRO FAILSAFE ELECTRONIC MODULE 4/8 F-DI/ 4 F-DO DC24V/2A PROFISAFE, 90 MM WIDTH, UP TO CATEGORY 4 (EN954-1)/ SIL3 (IEC61508)/PLE (ISO13849),",563,"TEM",1,"Simatic",0.32400000000000001,1]
["6ES71484FS000AB0","SIMATIC DP,  ET 200PRO FAILSAFE ELECTRONIC MODULE F-SWICH PROFISAFE, 3 FAILSAFE PP-SWITCHING OUTPUTS TO SAFELY SWITCH  THE BACKPLANE RAILS (2L+, F0, F1) 2 FAILSAFE DIGITALE INPUTS, 45 MM, UP TO CATEGORY 4 (EN954-1)/ SIL3 (IEC61508)/PLE (ISO13849),",367,"TEM",1,"Simatic",0.20200000000000001,1]
["6ES71486CB000AA0","SIMATIC DP, ET 200ECO PN, POWER DISTRIBUTOR PD DC 24V; 1 X 7/8\", 4 X M12, DEGREE OF PROTECTION IP67;",132,"TEM",1,"Simatic",0.63800000000000001,1]
["6ES71486JA000AB0","SIMATIC DP, ET 200ECO PN, IO-LINK MASTER, 4IO-L + 8DI + 4DO 24V DC/1.3A 8 X M12, DOUBLE-ASSIGNEMENT, DEGREE OF PROTECTION IP67",473,"TEM",1,"Simatic",0.98399999999999999,1]
["6ES71486JD000AB0","SIMATIC DP, ET 200eco PN, IO-Link maSTer, 4IO-L, 4 x M12, degree of protection IP67",415,"TEM",1,"Simatic",0.98399999999999999,1]
["6ES71511AA050AB0","SIMATIC DP, INTERFACE MODULE IM151-1 STANDARD FOR ET200S; INCL. TERMINATING MODULE DATA VOLUME 244BYTE FOR EACH INPUT AND OUTPUT; MAX. OF 63 PERIPHERIEMODULES PROFIBUS DP V0 AND V1 UP TO 2M WIDTH CONNECTABLE; BUS INTERFACING VIA 9-WAY SUB-D",253,"TEM",1,"Simatic",0.17299999999999999,1]
["6ES71511AA060AB0","SIMATIC DP, INTERFACE MODULE IM151-1 STANDARD FOR ET200S; INCL. TERMINATING MODULE DATA VOLUME 244BYTE FOR EACH INPUT AND OUTPUT; MAX. OF 63 PERIPHERIEMODULES PROFIBUS DP V0 AND V1 UP TO 2M WIDTH CONNECTABLE; BUS INTERFACING VIA 9-WAY SUB-D",253,"TEM",1,"Simatic",0.17299999999999999,1]
["6ES71511BA020AB0","SIMATIC DP, INTERFACE MODULE IM151-1 HIGH FEATURE F. ET200S; TRANSMISS. RATE UP TO 12MBIT/S; DATA VOLUMEN  244 BYTE FOR I/O, MAX. 63  MODULES CONNECTABLE; ISOCHRONE MODE, BUS INTERFACING VIA 9-WAY SUB-D CONNECTOR, INCL. TERMINATING MODULE",311,"TEM",1,"Simatic",0.17100000000000001,1]
["6ES71511CA000AB0","SIMATIC DP, INTERFACE MODULE IM151-1 BASIC FOR ET200S; TRANSMISS. RATE UP TO 12MBIT/S; MAX. OF 12 POWER, ELECTR. OR MOTOR STARTER MODULES (NO F-MODULES) CONNECTABLE; BUS INTERFACING VIA 9-WAY SUB-D CONN. INCL. TERMINATING MODULE",205,"TEM",1,"Simatic",0.16700000000000001,1]
["6ES71511CA001BL0","ET 200S COMPACT, 32DI STD, DC24V, 3MS, EXPANDABLE WITH UP TO 12 ET 200S MODULES (NO F-MODULES) ELECTRONICBLOCK",350,"TEM",1,"Simatic",0.28799999999999998,1]
["6ES71511CA003BL0","ET 200S COMPACT, 16DI/16DO STD DC24V, 3MS; DC24V, 0.5A EXPANDABLE WITH UP TO 12 ET 200S MODULES (NO F-MODULES) ELECTRONICBLOCK",396,"TEM",1,"Simatic",0.29299999999999998,1]
["6ES71513AA230AB0","SIMATIC DP, INTERFACE MODULE IM151-3 PN ST FOR ET200S; TRANSMISS. RATE UP TO 100MBIT/S MAX. OF 63 POWER, ELECTR. OR MOTOR STARTER MODULES UP TO 2M WIDTH CONNECTABLE; 2X BUS INTERFACING VIA RJ45 INCL. TERMINATING MODULE",253,"TEM",1,"Simatic",0.20100000000000001,1]
["6ES71513BA204AB1","ET 200S PN TRAINING BUNDLE IM151-3 PROFINET HIGH FEATURE 5X2DI DC24V A. 5X2DO DC24V/0.5A 2XPM-E 35MM DIN RAIL 483MM LENGTH 64KB MMC CARD FOR EDUCATIONAL PURPOSES ONLY OFFER LIMITED UNTIL 12-31-2015",717,"TEM",1,"Simatic",1.9,0]
["6ES71513BA230AB0","SIMATIC DP, INTERFACE MODULE IM151-3 PN HF FOR ET 200S, TRANSMISS. RATE UP TO 100MBIT/S MAX. OF 63 PERIPHERAL MODULES UP TO 2M WIDTH CONNECTABLE; 2 X BUS INTERFACING VIA RJ45 INCL. TERMINATING MODULE",311,"TEM",1,"Simatic",0.2,1]
["6ES71513BB230AB0","SIMATIC DP, INTERFACE MODULE IM151-3 PN FO FOR ET 200S 2 PROFINET FO INTERFACES INTEGRATED 2-PORT SWITCH MAX. OF 63 PERIPHERAL MODULES USABLE FOR PROFISAFE MODULES MAX. 2M STATION WIDTH INCL. TERMINATING MODULE",572,"TEM",1,"Simatic",0.24299999999999999,1]
["6ES71517AA210AB0","SIMATIC DP, IM151-7 CPU FOR ET200S, 128 KB WORKING MEMORY INTEGR. PROFIBUS DP INTERFACE (9 PIN SUB-D, FEMALE) AS DP SLAVE, W/O BATTERY SIMATIC MMC REQUIRED",662,"TEM",1,"Simatic",0.24399999999999999,1]
["6ES71517AB000AB0","SIMATIC DP, IM151-7 CPU FO FOR ET200S, WORKING MEMORY 48KB ( FROM FW V1.13 ON), INTEGR. PROFIBUS DP INTERFACE (FO SIMPLEX CONNECTOR) AS DP SLAVE, W/O BATTERY",678,"TEM",1,"Simatic",0.252,1]
["6ES71517FA210AB0","SIMATIC DP, IM151-7 F-CPU FOR ET200S, 192KB WORKING MEMORY WITH INTEGRATED PROFIBUS DP INTERFACE (9 PIN SUB-D, FEMALE) AS DP SLAVE, W/O BATTERY SIMATIC MMC REQUIRED",869,"TEM",1,"Simatic",0.25900000000000001,1]
["6ES71518AB010AB0","SIMATIC DP, IM151-8 PN/DP CPU FOR ET200S, 192 KB WORKING MEMORY, INT. PROFINET INTERFACE (WITH THREE RJ45 PORTS) AS IO-CONTROLER, W/O BATTERY MMC REQUIRED",698,"TEM",1,"Simatic",0.38700000000000001,1]
["6ES71518FB004AB1","TRAINING BUNDLE CPU IM 151-8F CONSISTING OF: IM151-8 F-CPU PN/DP, DP-MASTER INTERFACE, DIN RAIL 483MM (19\"), 5 X 4DI HF, 5 X 4DO HF, 2 X 2 AI U HF, 1 X 2 AO U HF, 1 X COUNT 24V/100KHZ, 2 X POWERMODUL PM-E RO, 1 X 4SI IO-LINK, 15 X UNIVERSAL TERMINALMODULE, MICRO MEMORY CARD 512 KBYTE, S7 DISTRIBUTED SAFETY V5.4 ******************************* FOR EDUCATIONAL PURPOSES ONLY OFFER LIMITED UNTIL 12-31-2015",1628,"TEM",1,"Simatic",3.5,0]
["6ES71518FB010AB0","SIMATIC DP, IM151-8F PN/DP CPU FOR ET200S, 256 KB WORKING MEMORY, INT. PROFINET INTERFACE (WITH THREE RJ45 PORTS) AS IO-CONTROLLER, W/O BATTERY MMC REQUIRED",1006,"TEM",1,"Simatic",0.39600000000000002,1]
["6ES71531AA030XB0","SIMATIC DP, INTERFACE IM 153-1, FOR ET 200M, FOR MAX. 8 S7-300 MODULES",278,"TEM",1,"Simatic",0.27400000000000002,1]
["6ES71532AR040XA0","SIMATIC DP, ET200M-RED.-BUNDLE CONSISTING OF: 2X IM153-2HF (6ES7153-2BA10-0XB0), 1X BUSMODULE IM/IM (6ES7195-7HD10-0XA0)",843,"TEM",1,"Simatic",0.71,0]
["6ES71532BA100XB0","SIMATIC DP, ET 200M INTERFACE IM 153-2 HIGH FEATURE FOR MAX. 12 S7-300 MODULES, WITH REDUNDANCY, TIME STAMPING FIT FOR ISOCHRONE MODE NEW FEATURES: 12 MODULES / STATION SLAVE INITIATIVE FOR  SWITCHES AND DRIVE ES EXTENDED DATA FOR HART SECON- DARY VARIABLES OPERATON WITH 64PT MODULES EXTENDES TIMESTAMPS WITH 32 SIGNALS / SLOT +++ SEE COMPATIBILITY NOTES IN IN THE MANUAL +++",422,"TEM",1,"Simatic",0.28399999999999997,1]
["6ES71532BA104AB1","TRAINING BUNDLE SIMATIC ET 200M/PCS7 PROFIBUS, CONSISTING OF: 1X INTERFACEMOD. IM153-2PB HF, 2X SM321, 32DI, 4X SM321, 16DI DIAG, 1X SM322, 32DO, 1X SM331, 8AI DIAG, 1X SM332, 8AO DIAG, 5X FRONT CONNECTOR SCREW 20PIN, 4 XFRONT CONNECT SCREW 40PIN, 1X RAIL 620MM, 6X BUS UNIT FOR IO MODULES, 1X BUS UNIT FOR  INTERFACEMOD., F. OPERATION 6ES7654-0UE23-0XS1 SIMATIC PCS 7 AS RTX - PROFIBUS NECESSARY, APPLICABLE FROM PCS 7 V8.0 SP2 ******************************* FOR EDUCATIONAL PURPOSES ONLY",796,"TEM",1,"Simatic",6.2,0]
["6ES71534AA010XB0","SIMATIC DP, ET 200M INTERFACE IM 153-4 PN IO FOR MAX. 12 S7-300 MODULES, EXTENDED FUNCTIONS: ISOCHRONEOUS REALTIME COMMUNICATION CLASS 1 AND 2, MODULE EXCHANGE W/O PG, OPERATION W/O MMC, MAINTENANCE NEW IO MODULES ARE SUPPORTED",278,"TEM",1,"Simatic",0.26,1]
["6ES71534BA000XB0","SIMATIC DP, ET 200M INTERFACE IM 153-4 PN IO HIGH FEATURE FOR MAX. 12 S7-300 MODULES, SUPPORTS FAIL SAFE MODULES, HART MODULES SHARED DEVICE, MEDIUM REDUNDANCY PROTOCOL",422,"TEM",1,"Simatic",0.26300000000000001,1]
["6ES71534BA004AB2","TRAINING BUNDLE SIMATIC ET 200M/PCS7 PROFINET, CONSISTING OF: 1X INTERFACEMOD. IM153-4PN HF, 2X SM321, 32DI, 4X SM321, 16DI DIAG, 1X SM322, 32DO, 1X SM331, 8AI DIAG, 1X SM332, 8AO DIAG, 5X FRONT CONNECTOR SCREW 20PIN, 4 XFRONT CONNECT SCREW 40PIN, 1X RAIL 620MM, 6X BUS UNIT FOR IO MODULES, 1X BUS UNIT FOR  INTERFACEMOD., F. OPERATION 6ES7654-0UE23-0XS2 SIMATIC PCS 7 AS RTX - PROFINET NECESSARY, APPLICABLE FROM PCS 7 V8.0 SP2 ******************************* FOR EDUCATIONAL PURPOSES ONLY",796,"TEM",1,"Simatic",6.2,0]
["6ES71541AA010AB0","SIMATIC DP, PROFIBUS DP INTERFACE MODULE IM154-1 DP FOR ET 200PRO INCLUSIVE TERMINATING MODULE, CONNECTING MODULE IM 6ES7194-4A.00-0AA0 MUST BE ORDERED SEPARATELY",188,"TEM",1,"Simatic",0.41,1]
["6ES71542AA010AB0","SIMATIC DP, PROFIBUS DP INTERFACE MODULE IM154-2 HIGH FEATURE FOR ET 200PRO INCLUSIVE TERMINATING MODULE, CONNECTING MODULE IM 6ES7194-4A.00-0AA0 MUST BE ORDERED SEPARATELY",268,"TEM",1,"Simatic",0.41,1]
["6ES71544AB100AB0","SIMATIC DP, PROFINET INTERFACE MODULE IM154-4 PN, HIGH FEATURE FOR ET 200PRO, INTEGRATED SWITCH, INCLUSIVE TERMINATING MODULE, CONNECTING MODULE IM PN 6ES7194-4A.00-0AA0 MUST BE ORDERED SEPARATELY",317,"TEM",1,"Simatic",0.54400000000000004,1]
["6ES71548AB010AB0","SIMATIC DP,  IM 154-8 PN/DP PLC FOR ET200PRO, 384KB WORK MEMORY, INT. PROFINET IF, INT.PROFIBUS DP MASTER/SLAVE IF PROT. IP65/67, MMC REQUIRED",1263,"TEM",1,"Simatic",0.77100000000000002,1]
["6ES71548FB010AB0","SIMATIC DP, IM 154-8F PN/DP PLC FOR ET200PRO, 512KB WORK MEMORY, INT. PROFINET IF, INT.PROFIBUS DP MASTER/SLAVE IF PROT. IP65/67, MMC REQUIRED",1756,"TEM",1,"Simatic",0.77100000000000002,1]
["6ES71548FX000AB0","SIMATIC DP, IM 154-8FX PN/DP CPU FOR ET200PRO, 1,5MB WORKING MEMORY, INT. PROFINET IF, INT.PROFIBUS DP MASTER/SLAVE IF PROT. IP65/67, MMC REQUIRED",3419,"TEM",1,"Simatic",0.76200000000000001,1]
["6ES71555AA000AB0","SIMATIC ET 200MP. PROFINET IO-DEVICE INTERFACEMODULE IM 155-5 PN ST FOR ET 200MP ELEKTRONIKMODULES; UP TO 12 IO-MODULES WITHOUT ADDITIONAL PS; UP TO 30 IO- MODULES WITH ADDITIONONAL PS SHARED DEVICE; MRP; IRT >=0.25MS; ISOCHRONICITY FW-UPDATE; I&M0...3; FSU WITH 500MS",396,"TEM",1,"Simatic",0.35899999999999999,1]
["6ES71555AA000AC0","SIMATIC ET 200MP. PROFINET IO-DEVICE INTERFACEMODULE IM 155-5 PN HF FOR ET 200MP ELEKTRONIKMODULES; UP TO 12 IO-MODULES WITHOUT ADDITIONAL PS; UP TO 30 IO- MODULES WITH ADDITIONONAL PS SHARED DEVICE; MRP; IRT >=0.25MS; ISOCHRONICITY FW-UPDATE; I&M0...3; FAST STARTUP S2 REDUNDANCY; SHARED DEV. WITH 4 CONTROLLER",460,"TEM",1,"Simatic",0.35599999999999998,1]
["6ES71555BA000AB0","SIMATIC ET 200MP. PROFIBUS INTERFACE MODULE IM155-5 DP ST FOR MAX. 12 S7-1500 MODULES",284,"TEM",1,"Simatic",0.39400000000000002,1]
["6ES71556AA000BN0","SIMATIC ET 200SP, BUNDLE PROFINET IM, IM155-6PN ST, MAX. 32 PERIPHERY MODULES AND 16 ET 200AL MODULES, SINGLE HOT SWAP, BUNDLE CONTAINS: INTERFACEMODULE (6ES7155-6AU00-0BN0), SERVERMODULE (6ES7193-6PA00-0AA0), BUSADAPTER BA 2X RJ45 (6ES7193-6AR00-0AA0)",279,"TEM",1,"Simatic",0.247,1]
["6ES71556AR000AN0","SIMATIC ET 200SP, PROFINET INTERFACE MODULE IM155-6PN BASIC, MAX. 12 PERIPHERY MODULES, 2X INTEGRATED RJ45 SOCKETS INCL. SERVERMODUL,",199,"TEM",1,"Simatic",0.24299999999999999,1]
["6ES71556AU000AB0","TRAINING BUNDLE SIMATIC ET 200SP BASIC CONSISTING OF: 1X INTERFACEMOD. IM155-6PN HF, 1X BUSADAPTER BA 2XRJ45, 2X DI 8X24VDC/0,5A HF, 2X DQ 8X24VDC/0,5A HF, 4X BASEUNITS, LABELING STRIPS, COLOUR CODED LABELS ******************************* FOR EDUCATIONAL PURPOSES ONLY",616,"TEM",1,"Simatic",1.5,0]
["6ES71556AU000AB1","TRAINING BUNDLE SIMATIC ET 200SP ENERGY METER CONSISTING OF: 1X INTERFACEMOD. IM155-6PN HF, 1X BUSADAPTER BA 2XRJ45, 2X DI 8X24VDC/0,5A HF, 2X DQ 8X24VDC/0,5A HF, 1X AI ENERGY METER ST, 5X BASEUNITS, SHIELD CONNECTORS, LABELING STRIPS, COLOUR CODED LABELS ******************************* FOR EDUCATIONAL PURPOSES ONLY",894,"TEM",1,"Simatic",1.6,0]
["6ES71556AU000AB2","TRAINING BUNDLE SIMATIC ET 200SP IO-LINK CONSISTING OF: 1X INTERFACEMOD. IM155-6PN HF, 1X BUSADAPTER BA 2XRJ45, 2X DI 8X24VDC/0,5A HF, 2X DQ 8X24VDC/0,5A HF, 1X CM 4XIO-LINK, 5X BASEUNITS, LABELING STRIPS, COLOUR CODED LABELS ******************************* FOR EDUCATIONAL PURPOSES ONLY",894,"TEM",1,"Simatic",1.4,0]
["6ES71556AU000AB3","TRAINING BUNDLE SIMATIC ET 200SP AS-I CONSISTING OF: 1X INTERFACEMOD. IM155-6PN HF, 1X BUSADAPTER BA 2XRJ45, 2X DI 8X24VDC/0,5A HF, 2X DQ 8X24VDC/0,5A HF, 1X CM AS-I, 5X BASEUNITS, LABELING STRIPS, COLOUR CODED LABELS ******************************* FOR EDUCATIONAL PURPOSES ONLY",1171,"TEM",1,"Simatic",1.4,0]
["6ES71556AU000AB6","TRAINING BUNDLE ANALOG FOR SIMATIC ET 200SP CONSISTING OF: 2X AI 2XU/I 2-/4-WIRE HS, 1X AQ 2XU/I HS, 3X BASEUNITS, SHIELD CONNECTORS, COLOUR CODED LABELS ******************************* FOR EDUCATIONAL PURPOSES ONLY",649,"TEM",1,"Simatic",0.3,0]
["6ES71556AU000BN0","SIMATIC ET 200SP, PROFINET INTERFACE MODULE IM155-6PN STANDARD, MAX. 32 PERIPHERY MODULES, INCL. SERVERMODUL",227,"TEM",1,"Simatic",0.20100000000000001,1]
["6ES71556AU000CN0","SIMATIC ET 200SP, PROFINET INTERFACE MODULE ET 200SP IM155-6PN HIGH FEATURE MAX. 64 PERIPHERY MODULES, 0.25 MS ISOCHRONOUS MODE MULTI HOT SWAP, INCL. SERVERMODUL",268,"TEM",1,"Simatic",0.2,1]
["6ES71556AU000DN0","SIMATIC ET 200SP, PROFINET INTERFACE MODULE IM155-6PN High Speed MAX. 30 PERIPHERY MODULES, 0.125 MS ISOCHRONOUS MODE MULTI HOT SWAP, INCL. SERVERMODUL",366,"TEM",1,"Simatic",0.2,1]
["6ES71556BA000CN0","SIMATIC ET 200SP, BUNDLE PROFIBUS IM, IM155-6DP HF, MAX. 32 PERIPHERY MODULES, AND 16 ET 200AL MODULES, MULTI HOT SWAP, BUNDLE CONTAINS: INTERFACEMODULE (6ES7 155-6BU00-0CN0), SERVER MODULE, (6ES7193-6PA00-0AA0), PROFIBUS CONNECTOR (6ES7972-0BB70-0XA0)",284,"TEM",1,"Simatic",0.23899999999999999,1]
["6ES71571AA000AB0","SIMATIC ET 200AL, PROFIBUS INTERFACEMODULE IM157-1 DP, DEGREE OF PROTECTION IP67",242,"TEM",1,"Simatic",0.248,1]
["6ES71571AB000AB0","SIMATIC ET 200AL, PROFNET INTERFACEMODULE IM157-1 PN, DEGREE OF PROTECTION IP67",242,"TEM",1,"Simatic",0.30499999999999999,1]
["6ES71580AD010XA0","SIMATIC DP, DISTRIBUTED I/O DP/DP COUPLER COUPLING MODULE  FOR CONNECTING TWO PROFIBUS DP NETWORKS REDUNDANTE POWERSUPPLY",515,"TEM",1,"Simatic",0.315,1]
["6ES71583AD010XA0","SIMATIC DP, DISTRIBUTED I/O PN/PN COUPLER COUPLING MODULE  FOR CONNECTING TWO PROFINET NETWORKS TRANSFER OF PROFISAFE DATA REDUNDANT POWERSUPPLY",625,"TEM",1,"Simatic",0.36499999999999999,1]
["6ES71740AA100AA0","SIMATIC S7-300,INTERFACE MODULE IM174, FOR CONNECTING ANALOG DRIVES AND STEP DRIVES VIA ISOCHRONUS PROFIBUS TO MOTION CONTROLLERS 4 CHANNELS (4 ENCOD.INP., 4 AO) CONFIGURABLE WITH STEP7 V5.4 SP4",873,"TEM",1,"Simatic",1.032,1]
["6ES71820AA010XA0","SIMATIC DP, IM 182-1 PC SLAVE BOARD FOR PROFIBUS DP, MAX. 12 MBIT/S",420,"TEM",1,"Simatic",0.2,1]
["6ES71934BA000AA0","10 DIN A4 LABELLING SHEETS COLOR: WHITE 60 LABELLING STRIPS/SHEETS FOR I/O MODULES AND 20 LABELLING STRIPS/SHEETS FOR INTERFACE MODULES MATERIAL: MEMBRANE, PREPERFO- RATED, FOR PRINTING ON A LASER PRINTER OR PLOTTER 10 SHEETS PER PACKAGING UNIT",55.900000000000006,"ΠΑΚ",1,"Simatic",0.14799999999999999,0]
["6ES71934BA100AA0","LABELING SHEETS BEIGE FOR ET 200 S COMPACT, DINA A4; FIT FOR AUTOMATIC PRINTIG WITH LASER PRINTERS OR PLOTTERS 10 PIECES PER PACKAGING UNIT",56.1,"ΠΑΚ",1,"Simatic",0.23400000000000001,0]
["6ES71934BB000AA0","10 DIN A4 LABELLING SHEETS COLOR: YELLOW 60 LABELLING STRIPS/SHEETS FOR I/O MODULES AND 20 LABELLING STRIPS/SHEETS FOR INTERFACE MODULES MATERIAL: MEMBRANE, PREPERFO- RATED, FOR PRINTING ON A LASER PRINTER OR PLOTTER 10 SHEETS PER PACKAGING UNIT",55.900000000000006,"ΠΑΚ",1,"Simatic",0.14399999999999999,0]
["6ES71934BB100AA0","LABELING SHEETS YELLOW FOR ET 200 S COMPACT, DINA A4; FIT FOR AUTOMATIC PRINTIG WITH LASER PRINTERS OR PLOTTERS 10 PIECES PER PACKAGING UNIT",56.1,"ΠΑΚ",1,"Simatic",0.22900000000000001,0]
["6ES71934BD000AA0","10 DIN A4 LABELLING SHEETS COLOR: RED 60 LABELLING STRIPS/SHEETS FOR I/O MODULES AND 20 LABELLING STRIPS/SHEETS FOR INTERFACE MODULES MATERIAL: MEMBRANE, PREPERFO- RATED, FOR PRINTING ON A LASER PRINTER OR PLOTTER 10 SHEETS PER PACKAGING UNIT",55.900000000000006,"ΠΑΚ",1,"Simatic",0.14899999999999999,0]
["6ES71934BD100AA0","LABELING SHEETS RED FOR ET 200 S COMPACT, DINA A4; FIT FOR AUTOMATIC PRINTIG WITH LASER PRINTERS OR PLOTTERS 10 PIECES PER PACKAGING UNIT",56.1,"ΠΑΚ",1,"Simatic",0.23599999999999999,0]
["6ES71934BH000AA0","10 DIN A4 LABELLING SHEETS COLOR: GREEN 60 LABELLING STRIPS/SHEETS FOR I/O MODULES AND 20 LABELLING STRIPS/SHEETS FOR INTERFACE MODULES MATERIAL: MEMBRANE, PREPERFO- RATED, FOR PRINTING ON A LASER PRINTER OR PLOTTER 10 SHEETS PER PACKAGING UNIT",55.900000000000006,"ΠΑΚ",1,"Simatic",0.14299999999999999,0]
["6ES71934BH100AA0","LABELING SHEETS PETROL FOR ET 200 S COMPACT, DINA A4; FIT FOR AUTOMATIC PRINTIG WITH LASER PRINTERS OR PLOTTERS 10 PIECES PER PACKAGING UNIT",56.1,"ΠΑΚ",1,"Simatic",0.23799999999999999,0]
["6ES71934CA200AA0","SIMATIC DP, 5 TERMINAL MODULES TM-E15S24-A1 FOR ET 200S FOR ELECTRONIC MODULES 15 MM WIDE,SCREW-TYPE TERMINALS 2X4 TERMINAL CONNECTIONS WITH TERMINAL LEAD TO AUX1, AUX1 IN LINE, 5 PIECES PER PACKAGING UNIT",38.6,"ΠΑΚ",1,"Simatic",0.375,1]
["6ES71934CA300AA0","SIMATIC DP, 5 TERMINAL MODULES TM-E15C24-A1 FOR ET 200S FOR ELECTRONIC MODULES 15MM WIDE,SPRING-LOAD TERMINALS 2X4 TERMINAL CONNECTIONS WITH TERMINAL LEAD TO AUX1, AUX1 IN LINE, 5 PIECES PER PACKAGING UNIT",38,"ΠΑΚ",1,"Simatic",0.32,1]
["6ES71934CA400AA0","SIMATIC DP, 5 UNIVERSAL TERMINAL MODULES TM-E15S26-A1 FOR ET 200S FOR ELECTRONIC MODULES 15MM WIDE, SCREW-TYPE TERMINALS 2X6 TERMINAL CONNECTIONS WITH TERMINAL LEAD TO AUX1, AUX1 IN LINE, 5 PIECES PER PACKAGING UNIT",50.400000000000006,"ΠΑΚ",1,"Simatic",0.46500000000000002,1]
["6ES71934CA500AA0","SIMATIC DP, 5 UNIVERSAL TERMINAL MODULES TM-E15C26-A1 FOR ET 200S FOR ELECTRONIC MODULES 15MM WIDE, CAGE CLAMP TERMINALS 2X6 TERMINAL CONNECTIONS WITH TERMINAL LEAD TO AUX1, AUX1 IN LINE, 5 PIECES PER PACKAGING UNIT",50.400000000000006,"ΠΑΚ",1,"Simatic",0.39200000000000002,1]
["6ES71934CA700AA0","SIMATIC DP, 5 TERMINAL MODULES TM-E15N24-A1 FOR ET 200S FOR ELECTRONIC MODULES 15MM WIDTH, FAST CONNECT TERMINAL, 2X4 TERMINAL CONNECTIONS WITH TERMINAL LEAD TO AUX1, AUX1 IN LINE, 5 PIECES PER PACKAGING UNIT",44.800000000000004,"ΠΑΚ",1,"Simatic",0.42699999999999999,1]
["6ES71934CA800AA0","SIMATIC DP, 5 UNIVERSAL TERMINAL MODULES TM-E15N26-A1 FOR ET 200S, FOR ELECTRONIC MODULES, 15MM WIDTH, FAST CONNECT TERMINAL, 2X6 TERMINAL CONNECTIONS WITH TERMINAL LEAD TO AUX1, AUX1 IN LINE, 5 PIECES PER PACKAGING UNIT",60.900000000000006,"ΠΑΚ",1,"Simatic",0.55400000000000005,1]
["6ES71934CB000AA0","SIMATIC DP, 5 TERMINAL MODULES TM-E15S23-01 FOR ET 200S FOR ELECTRONIC MODULES 15MM WIDE, SCREW-TYPE TERMINALS 2X3 TERMINAL CONNECTIONS W/O TERMINAL LEAD TO AUX1, AUX1 IN LINE, 5 PIECES PER PACKAGING UNIT",35.6,"ΠΑΚ",1,"Simatic",0.33200000000000002,1]
["6ES71934CB100AA0","SIMATIC DP, 5 TERMINAL MODULES TM-E15C23-01 FOR ET 200S FOR ELECTRONIC MODULES 15MM WIDE,SPRING-LOAD TERMINALS 2X3 TERMINAL CONNECTIONS W/O TERMINAL LEAD TO AUX1, AUX1 IN LINE, 5 PIECES PER PACKAGING UNIT",35,"ΠΑΚ",1,"Simatic",0.28000000000000003,1]
["6ES71934CB200AA0","SIMATIC DP, 5 TERMINAL MODULES TM-E15S24-01 FOR ET 200S FOR ELECTRONIC MODULES 15MM WIDE, SCREW-TYPE TERMINALS 2X4 TERMINAL CONNECTIONS W/O TERMINAL LEAD TO AUX1, AUX1 IN LINE, 5 PIECES PER PACKAGING UNIT",38.6,"ΠΑΚ",1,"Simatic",0.379,1]
["6ES71934CB300AA0","SIMATIC DP, 5 TERMINAL MODULES TM-E15C24-01 FOR ET 200S FOR ELECTRONIC MODULES 15MM WIDE,SPRING-LOAD TERMINALS 2X4 TERMINAL CONNECTIONS W/O TERMINAL LEAD TO AUX1, AUX1 IN LINE, 5 PIECES PER PACKAGING UNIT",38,"ΠΑΚ",1,"Simatic",0.34,1]
["6ES71934CB600AA0","SIMATIC DP, 5 TERMINAL MODULES TM-E15N23-01 FOR ET 200S FOR ELECTRONIC MODULES 15MM WIDTH, FAST CONNECT TERMINAL, 2X3 TERMINAL CONNECTIONS W/O TERMINAL LEAD TO AUX1, AUX1 IN LINE, 5 PIECES PER PACKAGING UNIT",41.400000000000006,"ΠΑΚ",1,"Simatic",0.38,1]
["6ES71934CB700AA0","SIMATIC DP, 5 TERMINAL MODULES TM-E15N24-01 FOR ET 200S FOR ELECTRONIC MODULES, 15MM WIDTH, FAST CONNECT TERMINAL, 2X4 TERMINAL CONNECTIONS W/O TERMINAL LEAD TO AUX1, AUX1 IN LINE, 5 PIECES PER PACKAGING UNIT",44.800000000000004,"ΠΑΚ",1,"Simatic",0.438,1]
["6ES71934CC200AA0","SIMATIC DP, TERMINAL MODULE TM-P15S23-A1 FOR ET 200S FOR POWER MODULES 15MM WIDE, SCREW-TYPE TERMINALS 2X3 TERMINAL CONNECTIONS WITH TERMINAL LEAD TO AUX1 AUX1 IN LINE",7.8000000000000007,"TEM",1,"Simatic",7.0999999999999994E-2,1]
["6ES71934CC201AA0","SIMATIC DP, 5 TERMINAL MODULES TM-P15S23-A1 FOR ET 200S FOR POWER MODULES 15MM WIDE, SCREW-TYPE TERMINALS 2X3 TERMINAL CONNECTIONS WITH TERMINAL LEAD TO AUX1 AUX1 IN LINE 5 PIECES PER PACKAGING UNIT",38.800000000000004,"ΠΑΚ",1,"Simatic",0.35499999999999998,0]
["6ES71934CC300AA0","SIMATIC DP, TERMINAL MODULE TM-P15C23-A1 FOR ET 200S FOR POWER MODULES 15MM WIDE,SPRING-LOAD TERMINALS (CAGE CLAMP), 2X3 TERMINAL CONNECTIONS WITH TERMINAL LEAD TO AUX1, AUX1 IN LINE",7.6000000000000005,"TEM",1,"Simatic",6.3E-2,1]
["6ES71934CC301AA0","SIMATIC DP, 5 TERMINAL MODULES TM-P15C23-A1 FOR ET 200S FOR POWER MODULES 15MM WIDE,SPRING-LOAD TERMINALS (CAGE CLAMP), 2X3 TERMINAL CONNECTIONS WITH TERMINAL LEAD TO AUX1, AUX1 IN LINE 5 PIECES PER PACKAGING UNIT",38.1,"ΠΑΚ",1,"Simatic",0.315,0]
["6ES71934CC700AA0","SIMATIC DP, TERMINAL MODULE TM-P15N23-A1 FOR ET 200S FOR POWER MODULES, 15MM WIDTH, FAST CONNECT TERMINAL, 2X3 TERMINAL CONNECTIONS WITH TERMINAL LEAD TO AUX1, AUX1 IN LINE",8.8000000000000007,"TEM",1,"Simatic",8.1000000000000003E-2,1]
["6ES71934CD200AA0","SIMATIC DP, TERMINAL MODULE TM-P15S23-A0 FOR ET 200S FOR POWER MODULES 15 MM WIDE,SCREW-TYPE TERMINALS 2X3 TERMINAL CONNECTIONS WITH TERMINAL LEAD TO AUX1 AUX1 INTERRUPTED",7.8000000000000007,"TEM",1,"Simatic",7.0000000000000007E-2,1]
["6ES71934CD201AA0","SIMATIC DP, 5 TERMINAL MODULES TM-P15S23-A0 FOR ET 200S FOR POWER MODULES 15 MM WIDE,SCREW-TYPE TERMINALS 2X3 TERMINAL CONNECTIONS WITH TERMINAL LEAD TO AUX1 AUX1 INTERRUPTED 5 PIECES PER PACKAGING UNIT",38.800000000000004,"ΠΑΚ",1,"Simatic",0.34499999999999997,0]
["6ES71934CD300AA0","SIMATIC DP, TERMINAL MODULE TM-P15C23-A0 FOR ET 200S FOR POWER MODULES 15MM WIDE,SPRING-LOAD TERMINALS (CAGE CLAMP), 2X3 TERMINAL CONNECTIONS WITH TERMINAL LEAD TO AUX1, AUX1 INTERRUPTED",7.6000000000000005,"TEM",1,"Simatic",6.3E-2,1]
["6ES71934CD301AA0","SIMATIC DP, 5 TERMINAL MODULES TM-P15C23-A0 FOR ET 200S FOR POWER MODULES 15MM WIDE,SPRING-LOAD TERMINALS (CAGE CLAMP), 2X3 TERMINAL CONNECTIONS WITH TERMINAL LEAD TO AUX1, AUX1 INTERRUPTED 5 PIECES PER PACKAGING UNIT",38.1,"ΠΑΚ",1,"Simatic",0.31,0]
["6ES71934CD700AA0","SIMATIC DP, TERMINAL MODULE TM-P15N23-A0 FOR ET 200S FOR POWER MODULES 15MM WIDE,FAST CONNECT TERMINAL 2X3 TERMINAL CONNECTIONS WITH TERMINAL LEAD TO AUX1, AUX1 INTERRUPTED",8.8000000000000007,"TEM",1,"Simatic",8.3000000000000004E-2,1]
["6ES71934CE000AA0","SIMATIC DP, TERMINAL MODULE TM-P15S22-01 FOR ET 200S FOR POWER MODULES 15 MM WIDE,SCREW-TYPE TERMINALS 2X2 TERMINAL CONNECTIONS W/O TERMINAL LEAD TO AUX1 AUX1 IN LINE",7.2,"TEM",1,"Simatic",6.3E-2,1]
["6ES71934CE001AA0","SIMATIC DP, 5 TERMINAL MODULES TM-P15S22-01 FOR ET 200S FOR POWER MODULES 15 MM WIDE,SCREW-TYPE TERMINALS 2X2 TERMINAL CONNECTIONS W/O TERMINAL LEAD TO AUX1 AUX1 IN LINE 5 PIECES PER PACKAGING UNIT",38.800000000000004,"ΠΑΚ",1,"Simatic",0.315,0]
["6ES71934CE100AA0","SIMATIC DP, TERMINAL MODULE TM-P15C22-01 FOR ET 200S FOR POWER MODULES 15MM WIDE,SPRING-LOAD TERMINALS (CAGE CLAMP), 2 X 2 TERMINAL CONNECTIONS W/O TERMINAL LEAD TO AUX1, AUX1 IN LINE",7,"TEM",1,"Simatic",5.7000000000000002E-2,1]
["6ES71934CE101AA0","SIMATIC DP, 5 TERMINAL MODULES TM-P15C22-01 FOR ET 200S FOR POWER MODULES 15MM WIDE,SPRING-LOAD TERMINALS (CAGE CLAMP), 2 X 2 TERMINAL CONNECTIONS W/O TERMINAL LEAD TO AUX1, AUX1 IN LINE 5 PIECES PER PACKAGING UNIT",38.1,"ΠΑΚ",1,"Simatic",0.28000000000000003,0]
["6ES71934CE600AA0","SIMATIC DP, TERMINAL MODULE TM-P15N22-01 FOR ET 200S FOR POWER MODULES, 15MM WIDTH, FAST CONNECT TERMINAL, 2X2 TERMINAL CONNECTIONS W/O TERMINAL LEAD TO AUX1, AUX1 IN LINE",8.8000000000000007,"TEM",1,"Simatic",7.1999999999999995E-2,1]
["6ES71934CF400AA0","SIMATIC DP, TERMINAL MODULE TM-E30S46-A1 FOR ET 200S FOR ELECTRONIC MODULES 30MM WIDE, SCREW-TYPE TERMINALS 4X6 TERMINAL CONNECTIONS WITH TERMINAL LEAD TO AUX1, AUX1 IN LINE,",33.4,"TEM",1,"Simatic",0.17699999999999999,1]
["6ES71934CF500AA0","SIMATIC DP, TERMINAL MODULE TM-E30C46-A1 FOR ET 200S FOR ELECTRONIC MODULES 30MM WIDE,SPRING-LOAD TERMINALS 4X6 TERMINAL CONNECTIONS WITH TERMINAL LEAD TO AUX1, AUX1 IN LINE,",32.800000000000004,"TEM",1,"Simatic",0.156,1]
["6ES71934CG200AA0","SIMATIC DP, 1 TERMINAL MODULE TM-E30S44-01 FOR ET 200S FOR ELECTRONIC MODULES 30MM WIDE, SCREW-TYPE TERMINALS 4X4 TERMINAL CONNECTIONS W/O TERMINAL LEAD TO AUX1, AUX1 IN LINE,",28.700000000000003,"TEM",1,"Simatic",0.14000000000000001,1]
["6ES71934CG300AA0","SIMATIC DP, 1 TERMINAL MODULE TM-E30C44-01 FOR ET 200S FOR ELECTRONIC MODULES 30MM WIDE,SPRING-LOAD TERMINALS 4X4 TERMINAL CONNECTIONS W/O TERMINAL LEAD TO AUX1, AUX1 IN LINE,",28.200000000000003,"TEM",1,"Simatic",0.11899999999999999,1]
["6ES71934CK200AA0","SIMATIC DP, TERMINAL MODULE TM-P30S44-A0 FOR ET 200S, FOR POWER MODULE PM-E F PROFISAFE, 30MM WIDE, SCREW-TYPE TERMINALS 2X3 + 2X4 TERMINAL CONNECTIONS WITH TERMINAL LEAD TO AUX1 AUX1 INTERRUPTED",29.200000000000003,"TEM",1,"Simatic",0.13300000000000001,1]
["6ES71934CK300AA0","SIMATIC DP, TERMINAL MODULE TM-P30C44-A0 FOR ET 200S, FOR POWER MODULE PM-E F PROFISAFE, 30MM WIDE,SPRING-LOAD TERMINALS 2X3 + 2X4 TERMINAL CONNECTIONS WITH TERMINAL LEAD TO AUX1 AUX1 INTERRUPTED",29.200000000000003,"TEM",1,"Simatic",0.115,1]
["6ES71934CL200AA0","SIMATIC DP, 1 TERMINAL MODULE TM-E15S24-AT FOR ET 200S FOR ELECTRONIC MODULE 2 AI TC HIGH FEATURE, 15 MM WIDE,SCREW-TYPE TERMINALS W/O TERMINAL LEAD TO AUX1, AUX1 IN LINE,",21.200000000000003,"TEM",1,"Simatic",6.9000000000000006E-2,1]
["6ES71934CL300AA0","SIMATIC DP, 1 TERMINAL MODULE TM-E15C24-AT FOR ET 200S FOR ELECTRONIC MODULE 2 AI TC HIGH FEATURE, 15MM WIDE,SPRING-LOAD TERMINALS TERMINAL LEAD TO AUX1, AUX1 IN LINE,",20.700000000000003,"TEM",1,"Simatic",6.4000000000000001E-2,1]
["6ES71934DL000AA0","SIMATIC DP, TERMINAL MODULE TM-C120C FOR ET 200S COMPACT, SPRING-LOADED TERMINALS, 4 X 21 CONNECTORS, FIT FOR 32PT MODULES IN 2-WIRE",56.300000000000004,"TEM",1,"Simatic",0.39300000000000002,1]
["6ES71934DL100AA0","SIMATIC DP, TERMINAL MODULE TM-C120S FOR ET 200S COMPACT, SCREW-TYPE TERMINALS, 4 X 21 CONNECTORS, FIT FOR 32PT MODULES IN 2-WIRE",56.300000000000004,"TEM",1,"Simatic",0.49,1]
["6ES71934FL000AA0","SIMATIC DP, ADDITIONAL TERM. FOR ET 200S AND ET 200S COMPACT 32PT IN 3 WIRE CLAMP-TYPE TERMINAL USE 2 ADDITIONAL TERMINALS FOR 4-WIRE",21.900000000000002,"TEM",1,"Simatic",0.16,1]
["6ES71934FL100AA0","SIMATIC DP, ADDITIONAL TERM. FOR ET 200S AND ET 200S COMPACT 32PT IN 3 WIRE SCREW-TYPE TERMINAL USE 2 ADDITIONAL TERMINALS FOR 4-WIRE",22.3,"TEM",1,"Simatic",0.20399999999999999,1]
["6ES71934GA000AA0","5 SHIELD CONNECTING ELEMENTS TERMINAL MODULES TM-P AND TM-E THE ET 200S AS RETAINING DEVICE FOR POWER RAIL 3 X 10 MM F. CONNECTION OF SHIELDED LEADS 5 PIECES PER PACKAGING UNIT",35,"ΠΑΚ",1,"Simatic",9.0000000000000011E-3,1]
["6ES71934GB000AA0","5 TERMINAL ELEMENTS F. ET 200S F.CONNECTION OF BRAIDED SHIELDS WITH THE POWER RAIL 5 PIECES PER PACKAGING UNIT",23.3,"ΠΑΚ",1,"Simatic",6.4000000000000001E-2,1]
["6ES71934JA000AA0","SIMATIC DP, SPARE PART TERMINATING MODULE FOR ET 200S",24.8,"TEM",1,"Simatic",2.3E-2,1]
["6ES71934JB000AA0","CONNECTOR, FEMALE, 2X2-PIN, 24 V DC FOR ET200S, INTERFACE MODULE, KP32F, PN/PN COUPLER, SPRING-LOADED TERMINALS, INTERNALLY BRIDGED, COLOR-CODED AMOUNT: SEE TECHNICAL DATA",26.3,"ΠΑΚ",1,"Simatic",4.9000000000000002E-2,1]
["6ES71934JB500AA0","SIMATIC DP, SPARE PART DC 24V PLUG FOR ET 200S INTERFACE MODULES UND PN/PN-COUPLER 2-POLES, SCREW-TYPE TERMINALS, FOR ELECTRONIC POWER SUPPLY 10 PIECES PER PACKAGING UNIT",27.700000000000003,"ΠΑΚ",1,"Simatic",6.0999999999999999E-2,1]
["6ES71934LA200AA0","200 COLOR CODING PLATES FOR TERMINAL MODULES OF THE ET 200S AND ET 200S COMPACT IN THE COLOR WHITE",13.4,"ΠΑΚ",1,"Simatic",1E-3,0]
["6ES71934LB200AA0","200 COLOR CODING PLATES FOR TERMINAL MODULES OF THE ET 200S AND ET 200S COMPACT IN THE COLOR YELLOW",13.4,"ΠΑΚ",1,"Simatic",1E-3,0]
["6ES71934LC200AA0","200 COLOR CODING PLATES FOR TERMINAL MODULES OF THE ET 200S AND ET 200S COMPACT IN THE COLOR YELLOW-GREEN",40.5,"ΠΑΚ",1,"Simatic",1E-3,0]
["6ES71934LD200AA0","200 COLOR CODING PLATES FOR TERMINAL MODULES OF THE ET 200S AND ET 200S COMPACT IN THE COLOR RED",13.4,"ΠΑΚ",1,"Simatic",1E-3,0]
["6ES71934LF200AA0","200 COLOR CODING PLATES FOR TERMINAL MODULES OF THE ET 200S AND ET 200S COMPACT IN THE COLOR BLUE",13.4,"ΠΑΚ",1,"Simatic",1E-3,0]
["6ES71934LG200AA0","200 COLOR CODING PLATES FOR TERMINAL MODULES OF THE ET 200S AND ET 200S COMPACT IN THE COLOR BROWN",13.4,"ΠΑΚ",1,"Simatic",1E-3,0]
["6ES71934LH200AA0","200 COLOR CODING PLATES FOR TERMINAL MODULES OF THE ET 200S AND ET 200S COMPACT IN THE COLOR TURQUOISE",13.4,"ΠΑΚ",1,"Simatic",1E-3,0]
["6ES71936AF000AA0","SIMATIC ET 200SP, BUSADAPTER BA 2XFC, 2X FAST CONNECT TERMINALS FOR PROFINET",62.2,"TEM",1,"Simatic",6.3E-2,1]
["6ES71936AG000AA0","SIMATIC BUSADAPTER BA 2XLC, 2 X LC GLASS-FO-CONNECTORS, FOR PROFINET",276,"TEM",1,"Simatic",6.3E-2,1]
["6ES71936AG200AA0","SIMATIC BUSADAPTER BA LC/RJ45, MEDIA CONVERTER FO - CU 1 X LC GLASS-FO-SOCKET AND, 1 X RJ45 SOCKET FOR PROFINET",213,"TEM",1,"Simatic",6.3E-2,1]
["6ES71936AG400AA0","SIMATIC BUSADAPTER BA LC/FC, MEDIA CONVERTER FO - CU 1 X LC GLASS-FO-SOCKET AND, 1 X FASTCONNECT (FC) SOCKET FOR PROFINET",223,"TEM",1,"Simatic",6.3E-2,1]
["6ES71936AP000AA0","SIMATIC ET 200SP, BUSADAPTER BA 2XSCRJ, 2 SCRJ FO-CONNECTORS, FOR PROFINET",276,"TEM",1,"Simatic",7.8E-2,1]
["6ES71936AP200AA0","SIMATIC ET 200SP, BUSADAPTER BA SCRJ/RJ45, MEDIA CONVERTER FO - CU 1 X SCRJ FO-SOCKET AND, 1 X RJ45 SOCKET FOR PROFINET",213,"TEM",1,"Simatic",0.05,1]
["6ES71936AP400AA0","SIMATIC ET 200SP, BUSADAPTER BA SCRJ/FC, MEDIA CONVERTER FO - CU 1 X SCRJ FO-SOCKET AND, 1 X FASTCONNECT (FC) SOCKET FOR PROFINET",223,"TEM",1,"Simatic",0.05,1]
["6ES71936AR000AA0","SIMATIC ET 200SP, BUSADAPTER BA 2X RJ45, 2 RJ45 SOCKETS FOR PROFINET",51.5,"TEM",1,"Simatic",5.5E-2,1]
["6ES71936AS000AA0","SIMATIC ET 200SP, BUSADAPTER BA-SEND BA1XFC, 1X FAST CONNECT TERMINAL FOR ET-CONNECTION",104,"TEM",1,"Simatic",5.2999999999999999E-2,1]
["6ES71936BN000NE0","SIMATIC ET 200SP, BASEUNIT BU-SEND FOR EXTENSION OF AN ET 200SP STATION VIA ET-CONNECTION WXH: 20MMX117MM",51.5,"TEM",1,"Simatic",0.04,1]
["6ES71936BP000BA0","SIMATIC ET 200SP, BASEUNIT BU15-P16+A0+2B, BU-TYPE A0, PUSH-IN TERMINALS, W/O AUX-TERMINALS, BRIDGED TO LEFT BU WXH: 15MMX117MM",14.100000000000001,"TEM",1,"Simatic",4.8000000000000001E-2,1]
["6ES71936BP000BA1","SIMATIC ET 200SP, BASEUNIT BU15-P16+A0+2B/T, BU-TYPE A1, PUSH-IN TERMINALS, W/O AUX-TERMINALS, BRIDGED TO LEFT BU, WXH: 15MMX117MM, WITH TEMPERATUR MEASURING",19.400000000000002,"TEM",1,"Simatic",4.9000000000000002E-2,1]
["6ES71936BP000BD0","SIMATIC ET 200SP, BASEUNIT BU20-P12+A0+0B, BU-TYPE D0, PUSH-IN KLEMMEN, W/O AUX-TERMINALS, BRIDGED TO LEFT BU WXH: 20MMX117MM",19.3,"TEM",1,"Simatic",5.5E-2,1]
["6ES71936BP000DA0","SIMATIC ET 200SP, BASEUNIT BU15-P16+A0+2D, BU-TYPE A0, PUSH-IN TERMINALS, W/O AUX-TERMINALS, NEW LOADGROUP, WXH: 15MMX117MM",24.8,"TEM",1,"Simatic",4.8000000000000001E-2,1]
["6ES71936BP000DA1","SIMATIC ET 200SP, BASEUNIT BU15-P16+A0+2D/T, BU-TYPE A1, PUSH-IN TERMINALS, W/O AUX-TERMINALS, NEW LOAD GROUP, WXH: 15MMX117MM, WITH TEMPERATURE MEASURING",30.200000000000003,"TEM",1,"Simatic",4.8000000000000001E-2,1]
["6ES71936BP002BA0","SIMATIC ET 200SP, BASEUNIT BU15-P16+A0+2B, BU-TYPE A0, PACKING UNIT: 10 PIECES, PUSH-IN TERMINALS, W/O AUX-TERMINALS, BRIDGED TO LEFT BU, WXH: 15MMX117MM",14.100000000000001,"TEM",1,"Simatic",0.4,0]
["6ES71936BP002DA0","SIMATIC ET 200SP, BASEUNIT BU15-P16+A0+2D, BU-TYPE A0, PACKING UNIT: 10 PIECES, PUSH-IN TERMINALS, W/O AUX-TERMINALS, NEW LOADGROUP, WXH: 15MMX117MM",24.8,"TEM",1,"Simatic",0.4,0]
["6ES71936BP200BA0","SIMATIC ET 200SP, BASEUNIT BU15-P16+A10+2B, BU-TYPE A0, PUSH-IN TERMINALS, WITH 10 AUX-TERMINALS, BRIDGED TO LEFT BU WXH: 15MMX141MM",18.8,"TEM",1,"Simatic",5.8999999999999997E-2,1]
["6ES71936BP200BB0","SIMATIC ET 200SP, BASEUNIT BU20-P12+A4+0B, BU-TYPE B0, PUSH-IN KLEMMEN, WITH 4 AUX-TERMINALS, BRIDGED TO LEFT BU WXH: 20MMX117MM",19.3,"TEM",1,"Simatic",5.7000000000000002E-2,1]
["6ES71936BP200BB1","SIMATIC ET 200SP, BASEUNIT BU20-P12+A0+4B, BU-TYPE B1, PUSH-IN KLEMMEN, W/O AUX-TERMINALS, BRIDGED TO LEFT BU WXH: 20MMX117MM",19.3,"TEM",1,"Simatic",5.7000000000000002E-2,1]
["6ES71936BP200BC1","SIMATIC ET 200SP, BASEUNIT TYP B0, BU20-P6+A2+4B BU-TYPE C1, PUSH-IN KLEMMEN, WITH 2 AUX-TERMINALS, BRIDGED TO LEFT BU WXH: 20MMX117MM",19.3,"TEM",1,"Simatic",5.6000000000000001E-2,1]
["6ES71936BP200BF0","SIMATIC ET 200SP, BASEUNIT BU20-P8+A4+0B, BU-TYPE F0, PUSH-IN KLEMMEN, WITH AUX-TERMINALS, BRIDGED TO LEFT BU WXH: 20MMX117MM",19.3,"TEM",1,"Simatic",5.7000000000000002E-2,1]
["6ES71936BP200DA0","SIMATIC ET 200SP, BASEUNIT BU15-P16+A10+2D, BU-TYPE A0, PUSH-IN TERMINALS, WITH 10 AUX-TERMINALS, NEW LOADGROUP, WXH: 15MMX141MM",29.5,"TEM",1,"Simatic",5.8999999999999997E-2,1]
["6ES71936BP200DC0","SIMATIC ET 200SP, BASEUNIT BU20-P6+A2+4D BU-TYPE C0, PUSH-IN KLEMMEN, WITH 2 AUX-TERMINALS, NEW LOADGROUP, WXH: 20MMX117MM",30.1,"TEM",1,"Simatic",5.6000000000000001E-2,1]
["6ES71936BP202BA0","SIMATIC ET 200SP, BASEUNIT BU15-P16+A10+2B, BU-TYPE A0, PACKING UNIT: 10 PIECES, PUSH-IN TERMINALS, WITH 10 AUX-TERMINALS, BRIDGED TO LEFT BU, WXH: 15MMX141MM",18.8,"TEM",1,"Simatic",0.5,0]
["6ES71936BP202BB0","SIMATIC ET 200SP, BASEUNIT BU20-P12+A4+0B, BU-TYPE B0, PACKING UNIT: 10 PIECES, PUSH-IN KLEMMEN, WITH 4 AUX-TERMINALS, BRIDGED TO LEFT BU, WXH: 20MMX117MM",19.3,"TEM",1,"Simatic",0.4,0]
["6ES71936BP202DA0","SIMATIC ET 200SP, BASEUNIT BU15-P16+A10+2D, BU-TYPE A0, PACKING UNIT: 10 PIECES, PUSH-IN TERMINALS, WITH 10 AUX-TERMINALS, NEW LOADGROUP, WXH: 15MMX141MM",29.5,"TEM",1,"Simatic",0.5,0]
["6ES71936BP400BA1","SIMATIC ET 200SP, BASEUNIT BU15-P16+A0+12B/T, BU-TYPE A1, PUSH-IN TERMINALS, WITH 2X 5 ADDITIONAL TERMINALS, BRIDGED TO LEFT BU BXH: 15MMX141MM, WITH TEMPERATUR MEASURING",24.1,"TEM",1,"Simatic",0.06,1]
["6ES71936BP400DA1","SIMATIC ET 200SP, BASEUNIT BU15-P16+A0+12D/T. BU-TYPE A1, PUSH-IN TERMINALS, WITH 2X 5 ADDITIONAL TERMINALS, NEW LOADGROUP, BXH: 15MMX141MM, WITH TEMPERATURE MEASURING",34.9,"TEM",1,"Simatic",5.8999999999999997E-2,1]
["6ES71936CP002MA0","SIMATIC ET 200SP, 10 COLOR IDENTIFICATION LABELS COLOR CODE CC00, FOR PERIPHERY MODULES, MODULE SPECIFIC, FOR 16 PUSH-IN TERMINALS",11.3,"ΠΑΚ",1,"Simatic",3.0000000000000001E-3,0]
["6ES71936CP012MA0","SIMATIC ET 200SP, 10 COLOR IDENTIFICATION LABELS COLOR CODE CC01, FOR PERIPHERY MODULES, MODULE SPECIFIC, FOR 16 PUSH-IN TERMINALS",11.3,"ΠΑΚ",1,"Simatic",7.0000000000000001E-3,0]
["6ES71936CP022MA0","SIMATIC ET 200SP, 10 COLOR IDENTIFICATION LABELS COLOR CODE CC02, FOR PERIPHERY MODULES, MODULE SPECIFIC, FOR 16 PUSH-IN TERMINALS",11.3,"ΠΑΚ",1,"Simatic",7.0000000000000001E-3,0]
["6ES71936CP032MA0","SIMATIC ET 200SP, 10 COLOR IDENTIFICATION LABELS COLOR CODE CC03, FOR PERIPHERY MODULES, MODULE SPECIFIC, FOR 16 PUSH-IN TERMINALS",11.3,"ΠΑΚ",1,"Simatic",7.0000000000000001E-3,0]
["6ES71936CP042MA0","SIMATIC ET 200SP, 10 COLOR IDENTIFICATION LABELS COLOR CODE CC04, FOR PERIPHERY MODULES, MODULE SPECIFIC, FOR 16 PUSH-IN TERMINALS",11.3,"ΠΑΚ",1,"Simatic",7.0000000000000001E-3,0]
["6ES71936CP052MA0","SIMATIC ET 200SP, 10 COLOR IDENTIFICATION LABELS COLOR CODE CC05, FOR PERIPHERY MODULES, MODULE SPECIFIC, FOR 16 PUSH-IN TERMINALS",11.3,"ΠΑΚ",1,"Simatic",7.0000000000000001E-3,0]
["6ES71936CP412MB0","SIMATIC ET 200SP, 10 COLOR IDENTIFICATION LABELS COLOR CODE CC41, FOR PERIPHERY MODULES, MODULE SPECIFIC, FOR 12 PUSH-IN TERMINALS",11.3,"ΠΑΚ",1,"Simatic",9.0000000000000011E-3,0]
["6ES71936CP422MB0","SIMATIC ET 200SP, 10 COLOR IDENTIFICATION LABELS COLOR CODE CC42, FOR PERIPHERY MODULES, MODULE SPECIFIC, FOR BU-TYPE F0",11.3,"ΠΑΚ",1,"Simatic",9.0000000000000011E-3,0]
["6ES71936CP512MC0","SIMATIC ET 200SP, 10 COLOR IDENTIFICATION LABELS COLOR CODE CC51, FOR PERIPHERY MODULES, MODULE SPECIFIC, FOR 12 PUSH-IN TERMINALS",11.3,"ΠΑΚ",1,"Simatic",6.0000000000000001E-3,0]
["6ES71936CP522MC0","SIMATIC ET 200SP, 10 COLOR IDENTIFICATION LABELS COLOR CODE CC52, FOR PERIPHERY MODULES, MODULE SPECIFIC, FOR BU-TYPE C0",11.3,"ΠΑΚ",1,"Simatic",6.0000000000000001E-3,0]
["6ES71936CP712AA0","SIMATIC ET 200SP, 10 COLOR IDENTIFICATION LABELS COLOR CODE CC71, FOR 10 AUX TERMINALS, FOR BU-TYPE A0, WITH PUSH-IN TERMINALS",11.3,"ΠΑΚ",1,"Simatic",6.0000000000000001E-3,0]
["6ES71936CP722AA0","SIMATIC ET 200SP, 10 COLOR IDENTIFICATION LABELS COLOR CODE CC72, FOR 10 AUX TERMINALS, FOR BU-TYPE A0, WITH PUSH-IN TERMINALS",11.3,"ΠΑΚ",1,"Simatic",6.0000000000000001E-3,0]
["6ES71936CP732AA0","SIMATIC ET 200SP, 10 COLOR IDENTIFICATION LABELS COLOR CODE CC73, FOR 10 AUX TERMINALS, FOR BU-TYPE A0, WITH PUSH-IN TERMINALS",11.3,"ΠΑΚ",1,"Simatic",6.0000000000000001E-3,0]
["6ES71936CP742AA0","SIMATIC ET 200SP, 10 COLOR IDENTIFICATION LABELS COLOR CODE CC74, FOR 2X 5 ADDITIONAL TERMINALS, FOR BU-TYPE A1, WITH PUSH-IN TERMINALS",11.3,"ΠΑΚ",1,"Simatic",6.0000000000000001E-3,0]
["6ES71936CP812AB0","SIMATIC ET 200SP, 10 COLOR IDENTIFICATION LABELS COLOR CODE CC81, FOR 4 AUX TERMINALS, FOR BU-TYPE B0, WITH PUSH-IN TERMINALS",11.3,"ΠΑΚ",1,"Simatic",5.0000000000000001E-3,0]
["6ES71936CP822AB0","SIMATIC ET 200SP, 10 COLOR IDENTIFICATION LABELS COLOR CODE CC82, FOR 4 AUX TERMINALS, FOR BU-TYPE B0, WITH PUSH-IN TERMINALS",11.3,"ΠΑΚ",1,"Simatic",5.0000000000000001E-3,0]
["6ES71936CP832AB0","SIMATIC ET 200SP, 10 COLOR IDENTIFICATION LABELS COLOR CODE CC83, FOR 4 AUX TERMINALS, FOR BU-TYPE B0, WITH PUSH-IN TERMINALS",11.3,"ΠΑΚ",1,"Simatic",5.0000000000000001E-3,0]
["6ES71936CP842AC0","SIMATIC ET 200SP, 10 COLOR IDENTIFICATION LABELS COLOR CODE CC84, FOR 2 AUX TERMINALS, FOR BU-TYPE C0, WITH PUSH-IN TERMINALS",11.3,"ΠΑΚ",1,"Simatic",6.0000000000000001E-3,0]
["6ES71936CP852AC0","SIMATIC ET 200SP, 10 COLOR IDENTIFICATION LABELS COLOR CODE CC85, FOR 2 AUX TERMINALS, FOR BU-TYPE C0, WITH PUSH-IN TERMINALS",11.3,"ΠΑΚ",1,"Simatic",6.0000000000000001E-3,0]
["6ES71936CP862AC0","SIMATIC ET 200SP, 10 COLOR IDENTIFICATION LABELS COLOR CODE CC86, FOR 2 AUX TERMINALS, FOR BU-TYPE C0, WITH PUSH-IN TERMINALS",11.3,"ΠΑΚ",1,"Simatic",6.0000000000000001E-3,0]
["6ES71936EF001AA0","SIMATIC DP, SPARE PART 5 E-CODING ELEMENTS TYPE F, USABLE FOR ET 200SP MODULES F-DI, F-DQ, F-PM-E; 5 PIECES PER PACKAGING UNIT",84.2,"ΠΑΚ",1,"Simatic",8.9999999999999993E-3,1]
["6ES71936EH001AA0","SIMATIC DP, SPARE PART 5 E-CODING ELEMENTS TYPE H, USABLE FOR ET 200SP MODULES AS-I SAFETY, IO-LINK 5 PIECES PER PACKAGING UNIT",84.2,"ΠΑΚ",1,"Simatic",1.0999999999999999E-2,1]
["6ES71936LA100AA0","SIMATIC ET 200SP, 1000 LABELING STRIPES, LIGHT GREY, 10 SHEETS DIN A4, PERFORATED, PAPER, 280G/M2",45.6,"TEM",1,"Simatic",0.19500000000000001,0]
["6ES71936LA100AG0","SIMATIC ET 200SP, 1000 LABELING STRIPES, YELLOW, 10 SHEETS DIN A4, PERFORATED, PAPER, 280G/M2",45.6,"TEM",1,"Simatic",0.187,0]
["6ES71936LF300AW0","SIMATIC ET 200SP, 160 EQUIPMET IDENTIFIER PLATES, 10 SHEETS (160 LABELS), FOR BA, BU, IM AND PERIPHERY MODULES",26.3,"ΠΑΚ",1,"Simatic",0.123,0]
["6ES71936LR100AA0","SIMATIC ET 200SP, 500 LABELING STRIPES, LIGHT GREY, ROLL WITH 500 LABELS",138,"TEM",1,"Simatic",0.20200000000000001,0]
["6ES71936LR100AG0","SIMATIC ET 200SP, 500 LABELING STRIPES, YELLOW, ROLL WITH 500 LABELS",138,"TEM",1,"Simatic",0.19900000000000001,0]
["6ES71936PA000AA0","SIMATIC ET 200SP, SPARE PART SERVERMODULE FOR ET 200SP",37.5,"TEM",1,"Simatic",2.5999999999999999E-2,1]
["6ES71936SC001AM0","SIMATIC ET 200SP, 5 SHIELDING TERMINALS AND 5 SHIELDING PLATES, FOR DIRECT CONNECTION",49.7,"ΠΑΚ",1,"Simatic",0.10299999999999999,0]
["6ES71941AB010XA0","SIMATIC DP, DISTRIBUTED I/O ET200 FREQUENCY CONVERTER CONNECTOR FOR MOTOR FEEDER SHIELDED HANQ8, ASSIGNMENT TO DESINA SPECIFICATIONS",72.8,"TEM",1,"Simatic",0.23400000000000001,1]
["6ES71941JB100XA0","SIMATIC DP, BLANK PLUG ECOFAST FOR ET200, 10 PIECES PER EACH PACKAGING UNIT",79.800000000000011,"ΠΑΚ",1,"Simatic",5.0999999999999997E-2,1]
["6ES71941KA010XA0","SIMATIC DP, Y CONNECTOR FOR DISTRIBUTED I/O ET 200 FOR THE DOUBLE WIRING OF I/O WITH ONE CABLE TO ET 200 5-PIN M12",12.9,"TEM",1,"Simatic",0.03,1]
["6ES71942AA000AA0","M8 POWER CONNECTOR, PIN INSERT, 4 PIN",16.8,"TEM",1,"Simatic",2.5999999999999999E-2,1]
["6ES71942AB000AA0","M8 CONNECTOR FOR ET-CONNECTION, 4 PIN, SHIELD",25.200000000000003,"TEM",1,"Simatic",2.5999999999999999E-2,1]
["6ES71942AC000AA0","M8 POWER CONNECTOR, SOCKET INSERT, 4 PIN",16.8,"TEM",1,"Simatic",0.02,1]
["6ES71942BA000AA0","IDENTIFICATION LABELS 10X5 MM RAL9016, CONSISTS OF 200  LABELS ON FRAME, 40 LABELS PER FRAME",21.700000000000003,"TEM",1,"Simatic",5.5E-2,0]
["6ES71942KA000AA0","ET-CONNECTION FAST CONNECT STRIPPING TOOL, TOOL FOR FAST STRIPPING OF THE ET-CONNECTION BUS CABLE",61.2,"TEM",1,"Simatic",9.1999999999999998E-2,0]
["6ES71942LH020AA0","BUS CABLE FOR ET-CONNECTION, PREASSEMBLED WITH 2 X M8 CONNECTORS, 4 CORE, SHIELDED, LENGTH 0,19M",20,"TEM",1,"Simatic",3.5000000000000003E-2,1]
["6ES71942LH021AA0","POWER CABLE M8, PREASSEMBLED WITH M8 PLUG AND M8 SOCKET, 4 CORE, LENGTH 0,19M",12.600000000000001,"TEM",1,"Simatic",0.03,1]
["6ES71942LH030AA0","BUS CABLE FOR ET-CONNECTION, PREASSEMBLED WITH 2 X M8 CONNECTORS, 4 CORE, SHIELDED, LENGTH 0,3M",20,"TEM",1,"Simatic",3.5000000000000003E-2,1]
["6ES71942LH030AB0","BUS CABLE FOR ET-CONNECTION, PREASSEMBLED WITH 2 X M8 CONNECTORS ANGLED, 4 CORE, SHIELDED, LENGTH 0,3M",22.1,"TEM",1,"Simatic",3.7999999999999999E-2,1]
["6ES71942LH031AA0","POWER CABLE M8, PREASSEMBLED WITH M8 PLUG AND M8 SOCKET, 4 CORE, LENGTH 0,3M",12.600000000000001,"TEM",1,"Simatic",0.03,1]
["6ES71942LH031AB0","POWER CABLE M8, PREASSEMBLED WITH M8 PLUG ANGLED AND M8 SOCKET ANGLED, 4 CORE, LENGTH 0,3M",14.700000000000001,"TEM",1,"Simatic",0.03,1]
["6ES71942LH100AA0","BUS CABLE FOR ET-CONNECTION, PREASSEMBLED WITH 2 X M8 CONNECTORS, 4 CORE, SHIELDED, LENGTH 1,0M",23.1,"TEM",1,"Simatic",6.3E-2,1]
["6ES71942LH100AB0","BUS CABLE FOR ET-CONNECTION, PREASSEMBLED WITH 2 X M8 CONNECTORS ANGLED, 4 CORE, SHIELDED, LENGTH 1,0M",25.200000000000003,"TEM",1,"Simatic",6.4000000000000001E-2,1]
["6ES71942LH101AA0","POWER CABLE M8, PREASSEMBLED WITH M8 PLUG AND M8 SOCKET, 4 CORE, LENGTH 1,0M",13.200000000000001,"TEM",1,"Simatic",5.8999999999999997E-2,1]
["6ES71942LH101AB0","POWER CABLE M8, PREASSEMBLED WITH M8 PLUG ANGLED AND M8 SOCKET ANGLED, 4 CORE, LENGTH 1,0M",15.3,"TEM",1,"Simatic",6.0999999999999999E-2,1]
["6ES71942LH200AA0","BUS CABLE FOR ET-CONNECTION, PREASSEMBLED WITH 2 X M8 CONNECTORS, 4 CORE, SHIELDED, LENGTH 2,0M",26.3,"TEM",1,"Simatic",0.10200000000000001,1]
["6ES71942LH200AB0","BUS CABLE FOR ET-CONNECTION, PREASSEMBLED WITH 2 X M8 CONNECTORS ANGLED, 4 CORE, SHIELDED, LENGTH 2,0M",29.400000000000002,"TEM",1,"Simatic",0.108,1]
["6ES71942LH200AC0","BUS CABLE FOR ET-CONNECTION, PREASSEMBLED ONE SIDE WITH M8 CONNECTOR, 4 CORE, SHIELDED, LENGTH 2,0M",21,"TEM",1,"Simatic",9.2999999999999999E-2,1]
["6ES71942LH201AA0","POWER CABLE M8, PREASSEMBLED WITH M8 PLUG AND M8 SOCKET, 4 CORE, LENGTH 2,0M",13.700000000000001,"TEM",1,"Simatic",0.10199999999999999,1]
["6ES71942LH201AB0","POWER CABLE M8, PREASSEMBLED WITH M8 PLUG ANGLED AND M8 SOCKET ANGLED, 4 CORE, LENGTH 2,0M",15.8,"TEM",1,"Simatic",0.10299999999999999,1]
["6ES71942LH201AC0","POWER CABLE M8, PREASSEMBLED ONE SIDE WITH M8 SOCKET, 4 CORE, LENGTH 2,0M",9.5,"TEM",1,"Simatic",9.6000000000000002E-2,1]
["6ES71942LH500AA0","BUS CABLE FOR ET-CONNECTION, PREASSEMBLED WITH 2 X M8 CONNECTORS, 4 CORE, SHIELDED, LENGTH 5,0M",34.700000000000003,"TEM",1,"Simatic",0.216,1]
["6ES71942LH500AB0","BUS CABLE FOR ET-CONNECTION, PREASSEMBLED WITH 2 X M8 CONNECTORS ANGLED, 4 CORE, SHIELDED, LENGTH 5,0M",37.800000000000004,"TEM",1,"Simatic",0.23200000000000001,1]
["6ES71942LH500AC0","BUS CABLE FOR ET-CONNECTION, PREASSEMBLED ONE SIDE WITH M8 CONNECTOR, 4 CORE, SHIELDED, LENGTH 5,0M",29.400000000000002,"TEM",1,"Simatic",0.20899999999999999,1]
["6ES71942LH501AA0","POWER CABLE M8, PREASSEMBLED WITH M8 PLUG AND M8 SOCKET, 4 CORE, LENGTH 5,0M",15.3,"TEM",1,"Simatic",0.23,1]
["6ES71942LH501AB0","POWER CABLE M8, PREASSEMBLED WITH M8 PLUG ANGLED AND M8 SOCKET ANGLED, 4 CORE, LENGTH 5,0M",17.400000000000002,"TEM",1,"Simatic",0.23100000000000001,1]
["6ES71942LH501AC0","POWER CABLE M8, PREASSEMBLED ONE SIDE WITH M8 SOCKET, 4 CORE, LENGTH 5,0M",11.600000000000001,"TEM",1,"Simatic",0.224,1]
["6ES71942LN100AA0","BUS CABLE FOR ET-CONNECTION, PREASSEMBLED WITH 2 X M8 CONNECTORS, 4 CORE, SHIELDED, LENGTH 10M",49.400000000000006,"TEM",1,"Simatic",0.40300000000000002,1]
["6ES71942LN100AB0","BUS CABLE FOR ET-CONNECTION, PREASSEMBLED WITH 2 X M8 CONNECTORS ANGLED, 4 CORE, SHIELDED, LENGTH 10M",52.5,"TEM",1,"Simatic",0.442,1]
["6ES71942LN100AC0","BUS CABLE FOR ET-CONNECTION, PREASSEMBLED ONE SIDE WITH M8 CONNECTOR, 4 CORE, SHIELDED, LENGTH 10M",44.1,"TEM",1,"Simatic",0.40100000000000002,1]
["6ES71942LN101AA0","POWER CABLE M8, PREASSEMBLED WITH M8 PLUG AND M8 SOCKET, 4 CORE, LENGTH 10M",20,"TEM",1,"Simatic",0.441,1]
["6ES71942LN101AB0","POWER CABLE M8, PREASSEMBLED WITH M8 PLUG ANGLED AND M8 SOCKET ANGLED, 4 CORE, LENGTH 10M",22.1,"TEM",1,"Simatic",0.439,1]
["6ES71942LN101AC0","POWER CABLE M8, PREASSEMBLED ONE SIDE WITH M8 SOCKET, 4 CORE, LENGTH 10M",16.8,"TEM",1,"Simatic",0.42299999999999999,1]
["6ES71942LN150AA0","BUS CABLE FOR ET-CONNECTION, PREASSEMBLED WITH 2 X M8 CONNECTORS, 4 CORE, SHIELDED, LENGTH 15M",65.100000000000009,"TEM",1,"Simatic",0.6,1]
["6ES71942LN150AB0","BUS CABLE FOR ET-CONNECTION, PREASSEMBLED WITH 2 X M8 CONNECTORS ANGLED, 4 CORE, SHIELDED, LENGTH 15M",68.3,"TEM",1,"Simatic",0.6,1]
["6ES71942LN150AC0","BUS CABLE FOR ET-CONNECTION, PREASSEMBLED ONE SIDE WITH M8 CONNECTOR, 4 CORE, SHIELDED, LENGTH 15M",59.900000000000006,"TEM",1,"Simatic",0.6,1]
["6ES71942LN151AA0","POWER CABLE M8, PREASSEMBLED WITH M8 PLUG AND M8 SOCKET, 4 CORE, LENGTH 15M",29.400000000000002,"TEM",1,"Simatic",0.66,1]
["6ES71942LN151AB0","POWER CABLE M8, PREASSEMBLED WITH M8 PLUG ANGLED AND M8 SOCKET ANGLED, 4 CORE, LENGTH 15M",31.5,"TEM",1,"Simatic",0.66,1]
["6ES71942LN151AC0","POWER CABLE M8, PREASSEMBLED ONE SIDE WITH M8 SOCKET, 4 CORE, LENGTH 15M",26.3,"TEM",1,"Simatic",0.66,1]
["6ES71943JA000AA0","SIMATIC DP, BLANK PLUG 7/8\" FOR ET 200, 10 PIECES PER PACKAGING UNIT",7.7,"ΠΑΚ",1,"Simatic",4.0000000000000001E-3,1]
["6ES71944AA000AA0","SIMATIC DP, CONNECTING MODULE FOR PROFIBUS INTERFACE MODULES ET 200PRO; ECOFAST CU, 2 X ECOFAST CONNECTION RS485, INTEGRATED ADRESS SETTING AND BUS TERMINATION FOR PROFIBUS DP",80.400000000000006,"TEM",1,"Simatic",0.22600000000000001,1]
["6ES71944AB000AA0","SIMATIC DP, COMPENSATION CONNECTOR M12 WITH PT1000 INTEGRATED TO COLD-JUNCTION COMPENSATION AT THE CONNECTION OF",26.8,"TEM",1,"Simatic",4.9000000000000002E-2,1]
["6ES71944AC000AA0","SIMATIC DP, CONNECTING MODULE FOR PROFIBUS INTERFACE MODULES ET 200PRO; DIRECT CONNECTION, INTEGRATED ADRESS SETTING AND BUS TERMINATION FOR PROFIBUS DP",69.7,"TEM",1,"Simatic",0.34200000000000003,1]
["6ES71944AD000AA0","SIMATIC DP, CONNECTING MODULE FOR PROFIBUS INTERFACE MODULES ET 200PRO; M12 / 7/8\", 2 X M12 AND 2 X 7/8\", INTEGRATED ADRESS SETTING AND BUS TERMINATION FOR PROFIBUS DP",75,"TEM",1,"Simatic",0.46500000000000002,1]
["6ES71944AF000AA0","SIMATIC DP, CONNECTING MODULE FOR PROFINET INTERFACE MODULES ET 200PRO; CONNECTOR 2XRJ45 2X POWER PLUG PUSH PULL FOR PROFINET PN",124,"TEM",1,"Simatic",0.37,1]
["6ES71944AG000AA0","SIMATIC DP, CONNECTING MODULE FOR PROFINET INTERFACE MODULES ET 200PRO; CONNECTOR 2XSCRJ FO 2X POWER PLUG PUSH PULL FOR PROFINET PN",258,"TEM",1,"Simatic",0.38,1]
["6ES71944AJ000AA0","SIMATIC DP, CONNECTING MODULE FOR PROFINET INTERFACE MODULES ET 200PRO; M12 / 7/8\", 2 X M12 AND 2 X 7/8\",",75,"TEM",1,"Simatic",0.61699999999999999,1]
["6ES71944AN000AA0","SIMATIC DP, CONNECTING MODULE FOR ET200PRO PLC IM154-8 PN/DP, 4 X M12 UND 2 X 7/8\" , FOR PROFINET AND PROFIBUS DP",120,"TEM",1,"Simatic",0.61699999999999999,1]
["6ES71944AP000AA0","SIMATIC DP, Connection module for ET200pro CPU 1516PRO-2 PN, 3 x M12 and 2 x 7/8\" for 2 x PROFINET",115,"TEM",1,"Simatic",0.61699999999999999,1]
["6ES71944BA000AA0","SIMATIC DP, CONNECTING MODULE FOR POWER  MODULES PM-E ET 200PRO ECOFAST CU DP, 1 X ECOFAST CONNECTION RS485",75,"TEM",1,"Simatic",0.14899999999999999,1]
["6ES71944BC000AA0","SIMATIC DP, CONNECTING MODULE FOR POWER  MODULES PM-E ET 200PRO DIRECT CONNECTION: UP TO 2 CABLE FITTINGS M20",69.7,"TEM",1,"Simatic",0.19600000000000001,1]
["6ES71944BD000AA0","SIMATIC DP, CONNECTING MODULE FOR POWER MODULES PM-E ET 200PRO 7/8\", 1 X 7/8\"",75,"TEM",1,"Simatic",0.155,1]
["6ES71944BE000AA0","SIMATIC DP, CONNECTING MODULE FOR POWER MODULES PM-E ET 200PRO PUSH PULL",129,"TEM",1,"Simatic",0.157,1]
["6ES71944BH000AA0","SIMATIC DP, CONNECTING MODULE FOR POWER  MODULES OUTPUT PM-O ET 200PRO, 2XPUSH PULL",129,"TEM",1,"Simatic",0.14799999999999999,1]
["6ES71944CA000AA0","SIMATIC DP, CONNECTING MODULE FOR DIGITAL AND ANALOG ELECTRONIC MODULES ET 200PRO 4 X M12",34.300000000000004,"TEM",1,"Simatic",0.35799999999999998,1]
["6ES71944CA100AA0","SIMATIC DP, CONNECTING MODULE FOR DIGITAL ELECTRONIC MODULES ET 200PRO, 4 X M12, PLASTIC VERSION",29,"TEM",1,"Simatic",0.154,1]
["6ES71944CA200AA0","SIMATIC DP, connecting module for IO-Link maSTer ET 200pro, 4 x M12, plaSTic version",29,"TEM",1,"Simatic",0.154,1]
["6ES71944CA500AA0","SIMATIC DP, CONNECTING MODULE FOR DIGITAL (4DO UND 4 DO HF) ELECTRONIC MODULES ET 200PRO 4 X M12 WITH 2 X M12 SINGLE-ASSIGNEMENT, 2 X M12 DOUBLE-ASSIGNEMENT",40.800000000000004,"TEM",1,"Simatic",0.36,1]
["6ES71944CB000AA0","SIMATIC DP, CONNECTING MDULE FOR DIGITAL ELECTRONIC MODULES ET 200PRO 8 X M12",48.2,"TEM",1,"Simatic",0.35,1]
["6ES71944CB100AA0","SIMATIC DP, CONNECTING MODULE FOR DIGITAL ELECTRONIC MODULES ET 200PRO, 8 X M12, PLASTIC VERSION",40.800000000000004,"TEM",1,"Simatic",0.154,1]
["6ES71944CB500AA0","SIMATIC DP, CONNECTING MDULE FOR DIGITAL ELECTRONIC MODULE 16 DI DC24V AND 4 DIO / 4DO DC24V/0,5A, ET200PRO, 8 X M12",75,"TEM",1,"Simatic",0.35899999999999999,1]
["6ES71944DA000AA0","SIMATIC DP,  ET200PRO CONNECTING MODULE FOR FAILSAFE ELECTRONIC MODULE F-SWITCH PROFISAFE",43.7,"TEM",1,"Simatic",0.37,1]
["6ES71944DC000AA0","SIMATIC DP,  ET200PRO CONNECTING MODULE FOR FAILSAFE ELECTRONIC MODULE 4/8 F-DI/4 F-DO DC24V/2A",87.4,"TEM",1,"Simatic",0.61699999999999999,1]
["6ES71944DD000AA0","SIMATIC DP,  ET200PRO CONNECTING MODULE FOR FAILSAFE ELECTRONIC MODULE 8/16 F-DI DC24V",87.4,"TEM",1,"Simatic",0.58299999999999996,1]
["6ES71944EB000AA0","SIMATIC DP, CONNECTING MDULE FOR DIGITAL ELECTRONIC MODULES ET 200PRO 8 X M8",48.2,"TEM",1,"Simatic",0.35799999999999998,1]
["6ES71944FA000AA0","SIMATIC DP, CONNECTING MODULE FOR DIGITAL ELECTRONIC MODULES ET 200PRO 1XM23",48.2,"TEM",1,"Simatic",0.19400000000000001,1]
["6ES71944FB000AA0","SIMATIC DP, CONNECTING MODULE FOR DIGITAL ELECTRONIC MODULES ET 200PRO 2XM12, 8-PIN;",48.2,"TEM",1,"Simatic",0.154,1]
["6ES71944GA000AA0","SIMATIC DP, MODULE CARRIER NARROW VERSION FOR IO MODULES ET 200PRO, LENGTH: 500 MM",30,"TEM",1,"Simatic",1.59,1]
["6ES71944GA200AA0","SIMATIC DP, MODULE CARRIER NARROW VERSION FOR IO MODULES ET 200PRO SOLD BY THE METER, CONFIGURABLE BY THE USER, LENGTH: 2000 MM",77.100000000000009,"TEM",1,"Simatic",6.3689999999999998,1]
["6ES71944GA600AA0","SIMATIC DP, MODULE CARRIER NARROW VERSION FOR IO MODULES ET 200PRO LENGTH: 1000 MM, NEW  HOLE PATTERN",53.6,"TEM",1,"Simatic",3.16,1]
["6ES71944GB000AA0","SIMATIC DP, MODULE CARRIER WIDE VERSION FOR IO MODULES AND MOTORSTARTERS ET 200PRO, LENGTH: 500 MM",59,"TEM",1,"Simatic",2.3319999999999999,0]
["6ES71944GB200AA0","SIMATIC DP, MODULE CARRIER WIDE VERSION FOR IO MODULES AND MOTORSTARTERS ET 200PRO, SOLD BY THE METER, CONFIGURABLE BY THE USER, LENGTH: 2000 MM",144,"TEM",1,"Simatic",9.6999999999999993,0]
["6ES71944GB600AA0","SIMATIC DP, MODULE CARRIER WIDE VERSION FOR IO MODULES AND MOTORSTARTERS ET 200PRO, LENGTH: 1000 MM NEW HOLE PATTERN",97.5,"TEM",1,"Simatic",4.76,0]
["6ES71944GC200AA0","SIMATIC DP, MODULE CARRIER COMPACT VERSION FOR IO MODULES ET 200PRO, SOLD BY THE METER, CONFIGURABLE BY THE USER, LENGTH: 2000 MM",85.7,"TEM",1,"Simatic",6.58,1]
["6ES71944GC600AA0","SIMATIC DP, MODULE CARRIER COMPACT VERSION FOR IO MODULES ET 200PRO LENGTH: 1000 MM NEW HOLE PATTERN",57.900000000000006,"TEM",1,"Simatic",6.0970000000000004,1]
["6ES71944GC700AA0","SIMATIC DP, MODULE CARRIER COMPACT VERSION FOR IO MODULES ET 200PRO, LENGTH: 500 MM, NEW HOLE PATTERN",34.300000000000004,"TEM",1,"Simatic",1.6,0]
["6ES71944GD000AA0","SIMATIC DP, MODULE CARRIER COMPACT WIDE VERSION FOR IO MODULES AND MOTORSTARTERS ET 200PRO, LENGTH: 500 MM",61.1,"TEM",1,"Simatic",2.536,0]
["6ES71944GD100AA0","SIMATIC DP, MODULE CARRIER COMPACT WIDE VERSION FOR IO MODULES AND MOTORSTARTERS ET 200PRO, LENGTH: 1000 MM",99.7,"TEM",1,"Simatic",5.0679999999999996,0]
["6ES71944GD200AA0","SIMATIC DP, MODULE CARRIER COMPACT WIDE VERSION FOR IO MODULES AND MOTORSTARTERS ET 200PRO, SOLD BY THE METER, CONFIGURABLE BY THE USER, LENGTH: 2000 MM",146,"TEM",1,"Simatic",10.135999999999999,0]
["6ES71944HA000AA0","SIMATIC DP, MODULE LABELS FOR ET 200PRO TO MARK THE CONNECTION MODULES IO IN TERMS OF COLOUR; PACKAGE EACH WITH 100 LABELS 20 X 7 IN THE COLOURS RED, GREEN, BLUE, WHITE, YELLOW",62.2,"ΠΑΚ",1,"Simatic",0.10299999999999999,0]
["6ES71944HB000AA0","SIMATIC DP, FUSES 12.5A (SPARE PART) FOR ET 200PRO 10 PIECES PER PACKAGING UNIT",20.900000000000002,"ΠΑΚ",1,"Simatic",1.2E-2,1]
["6ES71944JA500AA0","SIMATIC DP, PROFINET IO CAPS FOR PUSH PULL SOCKETS (1L+; 2L+) POWER, 5 PIECES PER PACKAGING UNIT",64.3,"ΠΑΚ",1,"Simatic",0.16900000000000001,1]
["6ES71944JD500AA0","SIMATIC DP, PROFINET IO CAPS FOR PUSH PULL SOCKETS (SC RJ), 5 PIECES PER PACKAGING UNIT",59,"ΠΑΚ",1,"Simatic",9.9000000000000005E-2,1]
["6ES71944JD600AA0","SIMATIC DP, BLANK PLUG M12 WITH INSIDE THREAD, FOR PROTECTION OF PROFIBUS- INTERFACE  X01/DP1 AT ET 200PRO IM154-8 PN/DP CPU, 5 PIECES PER PACKAGING UNIT",13.4,"ΠΑΚ",1,"Simatic",1.7000000000000001E-2,1]
["6ES71946CA000AA0","SIMATIC DP,  PROFINET TERMINAL BLOCK FOR ET200ECO PN, 10A CUTTER CLAMPS",68.3,"TEM",1,"Simatic",0.1,1]
["6ES71946GA000AA0","SIMATIC DP,  PROFINET MOUNTING BAR  FOR ET200ECO PN LENGTHS 0,5M",52.5,"TEM",1,"Simatic",2.06,1]
["6ES71946HB000AA0","SIMATIC DP,  PROFINET REPLACEMENT FUSE FOR TERMINAL BLOCK ET200ECO PN 10 PIECES PER PACKAGING UNIT",10.5,"ΠΑΚ",1,"Simatic",7.0000000000000001E-3,1]
["6ES71946KA000XA0","SIMATIC DP, Y CABLE FOR DISTRIBUTED I/O ET 200 FOR THE DOUBLE WIRING OF I/O WITH ONE CABLE TO ET 200 5-PIN M12, 200MM",25.8,"TEM",1,"Simatic",5.8999999999999997E-2,1]
["6ES71946MA000AA0","SIMATIC DP,  PROFINET SELF-TAPPING SCREW FOR MOUNTING BAR ET200ECO PN 50 PIECES PER PACKAGING UNIT",15.8,"ΠΑΚ",1,"Simatic",0.27500000000000002,1]
["6ES71950AA050XA0","DP, ASIC ASPC2 STEP E2 LEADFREE FOR PROFIBUS DP, MASTER, MAX. 12 MBIT/S 6 UNITS FOR LABORATORY DEVELOPMENT",189,"ΠΑΚ",1,"Simatic",0.42599999999999999,0]
["6ES71950AA150XA0","DP, ASIC ASPC2 STEP E2 LEADFREE FOR PROFIBUS DP, MASTER, MAX. 12 MBIT/S 66 UNITS/TRAY",1824,"ΠΑΚ",1,"Simatic",0.52700000000000002,0]
["6ES71950AA250XA0","DP, ASIC ASPC2 STEP E2 LEADFREE FOR PROFIBUS DP, MASTER, MAX. 12 MBIT/S 660 UNITS/TRAY BOX",15433,"ΠΑΚ",1,"Simatic",2.7829999999999999,0]
["6ES71950BA020XA0","SIMATIC DP, ASIC LSPM2 LEADFREE FOR PROFIBUS DP, SLAVE, MAX. 12 MBITS/S, 32 I/O 6 FOR LABORATORY DEVELOPMENT",99.800000000000011,"ΠΑΚ",1,"Simatic",0.40400000000000003,0]
["6ES71950BA120XA0","SIMATIC DP, ASIC LSPM2 LEADFREE FOR PROFIBUS DP, SLAVE, MAX. 12 MBITS/S, 32 I/O 66 PCS./TRAY",965,"ΠΑΚ",1,"Simatic",0.51500000000000001,0]
["6ES71950BA220XA0","SIMATIC DP, ASIC LSPM2 LEADFREE FOR PROFIBUS DP, SLAVE, MAX. 12 MBITS/S, 32 I/O 330 PCS./1 TRAY-BOX",4091,"ΠΑΚ",1,"Simatic",1.6060000000000001,0]
["6ES71950BD040XA0","DP, ASIC SPC3 STEPC LEADFREE FOR PROFIBUS DP, MAX. 12 MBAUD 6 FOR LABORATORY DEVELOPMENT",116,"ΠΑΚ",1,"Simatic",0.45700000000000002,0]
["6ES71950BD140XA0","DP, ASIC SPC3, STEPC LEADFREE FOR PROFIBUS DP, MAX. 12 MBAUD 96 PCS. / 1 TRAY",1148,"ΠΑΚ",1,"Simatic",0.496,0]
["6ES71950BD240XA0","DP, ASIC SPC3 STEPC LEADFREE FOR PROFIBUS DP, MAX. 12 MBAUD 960 PCS. / 1 TRAY - BOX",9476,"ΠΑΚ",1,"Simatic",2.298,0]
["6ES71950BD440XA0","DP, ASIC SPC 3 STEP C LEADFREE FOR PROFIBUS DP, MAX. 12 MBAUD 750 PIECES T & R",7560,"ΠΑΚ",1,"Simatic",1.2170000000000001,0]
["6ES71950BE020XA0","DP, ASIC DPC31  STEPB LEADFREE FOR PROFIBUS DP, SLAVE ASIC W. PROCESSOR KERNEL 6 FOR LABORATORY DEVELOPMENT",99.800000000000011,"ΠΑΚ",1,"Simatic",0.56200000000000006,0]
["6ES71950BE120XA0","DP, ASIC, DPC31 STEPB LEADFREE FOR PROFIBUS DP, SLAVE ASIC W. PROCESSOR KERNEL 60 PCS. 1 TRAY",921,"ΠΑΚ",1,"Simatic",0.63700000000000001,0]
["6ES71950BE220XA0","DP,  ASIC DPC31  STEPB LEADFREE FOR PROFIBUS DP, SLAVE ASIC W. PROCESSOR KERNEL 300 PCS., 1 TRAY BOX",3898,"ΠΑΚ",1,"Simatic",1.84,0]
["6ES71950BF020XA0","DP, ASIC DPC31 STEP C1 LEADFREE FOR PROFIBUS DP, SLAVE ASIC W. PROCESSOR KERNEL, 6 PCS. FOR LABORATORY DEVELOPM. ++ PLEASE NOTE: NOT COMPATIBLE WITH DPC31 / STEP B ++",99.800000000000011,"ΠΑΚ",1,"Simatic",0.41299999999999998,0]
["6ES71950BF120XA0","DP, ASIC DPC31 STEP C1 LEADFREE FOR PROFIBUS DP, SLAVE ASIC W. PROCESSOR KERNEL 66 PCS. SINGLE TRAY +++ PLEASE NOTE: NOT COMPATIBLE WITH DPC31 / STEP B +++",912,"ΠΑΚ",1,"Simatic",0.54600000000000004,0]
["6ES71950BF220XA0","DP, ASIC DPC31 STEP C1 LEADFREE FOR PROFIBUS DP, SLAVE ASIC W. PROCESSOR KERNEL 660 PCS. TRAY BOX +++ PLEASE NOTE: NOT COMPATIBLE WITH DPC31 / STEP B +++",7717,"ΠΑΚ",1,"Simatic",2.8929999999999998,0]
["6ES71950BG000XA0","DP, ASIC SPC3LV (3,3V) LEADFREE FOR PROFIBUS DP, MAX. 12 MBAUD 5 FOR LABORATORY DEVELOPMENT",89.300000000000011,"ΠΑΚ",1,"Simatic",0.498,0]
["6ES71950BG100XA0","DP, ASIC SPC3LV (3,3V) LEADFREE FOR PROFIBUS DP, MAX. 12 MBAUD 160 PCS. / 1 TRAY",1680,"ΠΑΚ",1,"Simatic",0.499,0]
["6ES71950BG200XA0","DP, ASIC SPC3LV (3,3V) LEADFREE FOR PROFIBUS DP, MAX. 12 MBAUD 800 PCS. / 1 TRAY BOX",7560,"ΠΑΚ",1,"Simatic",1.41,0]
["6ES71950BG400XA0","DP, ASIC SPC3LV (3,3V) LEADFREE FOR PROFIBUS DP, MAX. 12 MBAUD 1000 PCS. T & R",9135,"ΠΑΚ",1,"Simatic",1.1759999999999999,0]
["6ES71950BH000XA0","ERTEC 200P, PROFINET IO ASIC, INDUSTRIAL ETHERNET 100 MBIT/S, ASIC WITH ARM PROCESSOR, 2-PORT SWITCH, PHY INTEGRATED, LEADFREE, DRYPACK 10 PIECES",392,"ΠΑΚ",1,"Simatic",0.39600000000000002,0]
["6ES71950BH100XA0","ERTEC 200P, PROFINET IO ASIC, INDUSTRIAL ETHERNET 100 MBIT/S, ASIC WITH ARM PROCESSOR, 2-PORT SWITCH, PHY INTEGRATED, LEADFREE, DRYPACK (1 TRAY) 90 PIECES",2205,"ΠΑΚ",1,"Simatic",0.46800000000000003,0]
["6ES71950BH200XA0","ERTEC 200P, PROFINET IO ASIC, INDUSTRIAL ETHERNET 100 MBIT/S, ASIC WITH ARM PROCESSOR, 2-PORT SWITCH, PHY INTEGRATED, LEADFREE, DRYPACK (5 TRAYS) 450 PIECES",10286,"ΠΑΚ",1,"Simatic",1.25,0]
["6ES71950BH300XA0","ERTEC 200P, PROFINET IO ASIC, INDUSTRIAL ETHERNET 100 MBIT/S, ASIC WITH ARM PROCESSOR, 2-PORT SWITCH, PHY INTEGRATED, LEADFREE, 1000 PCS. T & R",19821,"ΠΑΚ",1,"Simatic",2.5,0]
["6ES71951GA000XA0","SIMATIC DP, RAIL FOR ET 200M 483 MM LONG F. MAX. 5 BUS MOD. FUNCTION: INSERT/REMOVE",47.800000000000004,"TEM",1,"Simatic",1.208,0]
["6ES71951GC000XA0","SIMATIC DP, RAIL FOR ET 200M 2000 MM LONG FOR BUS MODULES FUNCTION: INSERT/REMOVE",168,"TEM",1,"Simatic",5.1349999999999998,0]
["6ES71951GF300XA0","SIMATIC DP, RAIL FOR ET 200M 530 MM LONG F. MAX. 5 BUS MOD. FUNCTION: INSERT/REMOVE",52.800000000000004,"TEM",1,"Simatic",1.34,0]
["6ES71951GG300XA0","SIMATIC DP, RAIL FOR ET 200M 620 MM LONG FOR BUS MODULES FUNCTION: INSERT/REMOVE",59.900000000000006,"TEM",1,"Simatic",1.56,0]
["6ES71951JA000XA0","SIMATIC DP, COVERS FOR BUS UNIT ET 200M,4 BACKPLANE BUS COVERS, 1 BUS BACKPLANE COVER,FUNCTION: INSERT/REMOVE",10.600000000000001,"TEM",1,"Simatic",1.7000000000000001E-2,1]
["6ES71951KA000XA0","SIMATIC DP, EXPLOSION-PROOF PARTITION PLATE FOR ET 200M TO PLUG IN TO A BUS MODULE FUNCTION: INSERT/REMOVE",13.200000000000001,"TEM",1,"Simatic",4.2999999999999997E-2,1]
["6ES71952BA000XA0","SIMATIC DP, FIRMWARE FOR ASIC SPC3 AND IM 182, SLAVE SOFTWARE FOR PROFIBUS DP, SOURCE CODE 6KB",1182,"TEM",1,"Simatic",0.2,0]
["6ES71952BA010XA0","SIMATIC DP, FIRMWARE FOR ASIC SPC3 AND IM 182, DP/V1 SLAVE SOFTWARE FOR PROFIBUS DP, SOURCE CODE APPR. 470 KB",2067,"TEM",1,"Simatic",0.21299999999999999,0]
["6ES71952BA020XA0","SIMATIC DP, FIRMWARE UPGRADE FOR ASIC SPC3 AND IM 182, SLAVE SOFTWARE UPGRADE FROM DP TO DP/V1 SOURCE CODE APPR. 470 KB",887,"TEM",1,"Simatic",0.13800000000000001,0]
["6ES71952BB000XA0","SIMATIC DP, FIRMWARE FOR ASIC DPC31, DP/V1 SLAVE SOFTWARE FOR PROFIBUS DP, SOURCE CODE APPR. 500 KB",2067,"TEM",1,"Simatic",0.215,0]
["6ES71953AA000YA0","PROFINET DRIVER FOR CONTROLLER DEVELOPMENT PACKAGE FOR PROFINET IO CONTROLLER V1.1, ON CD, SOURCE CODE WITH EXEMPLARY IMPLEMENTATION ON WINDOWS AND LINUX",735,"TEM",1,"Simatic",0.22600000000000001,0]
["6ES71953AA050XA0","RUNTIME LICENSE PROFINET DRIVER 1 PIECE, STICKER, LICENSE ONLY, NO SOFTWARE",572,"TEM",1,"Simatic",0.02,0]
["6ES71953AA100XA0","RUNTIME LICENSE PROFINET DRIVER 10 PIECES, STICKERS, LICENSE ONLY, NO SOFTWARE",3266,"TEM",1,"Simatic",2.1999999999999999E-2,0]
["6ES71953AA200XA0","RUNTIME LICENSE PROFINET DRIVER 50 PIECES, STICKERS, LICENSE ONLY, NO SOFTWARE",12245,"TEM",1,"Simatic",2.5999999999999999E-2,0]
["6ES71953BC100YA0","PRODUCTLINE LICENSE FOR PN IO FW-STACK",8000,"TEM",1,"Simatic",4.2999999999999997E-2,0]
["6ES71953BE004AB1","TRAINER PACKAGE PROFINET & PROFISAFE, CONSISTING OF: EK-ERTEC 200P PN IO, EB200P, DOCUMENTATION, PN TREIBER FOR CONTROLLER, ETHERNET CABLE RJ45/RJ45 6M, PN IO DEVICE STACK, PROFISAFE-STARTERKIT V3.5, PROFISAFE DRIVER-SOFTWARE, IPARSERVER, TOOL-CALLING-INTERF EXAMPLE FOR EK-ERTEC 200P, BEISPIELE F. PN TREIBER (WINDOWS & LINUX) ******************************* FOR EDUCATIONAL PURPOSES ONLY",1106,"TEM",1,"Simatic",1,0]
["6ES71953BF020YA0","PROFISAFE-STARTERKIT V3.4 (FOR V1-MODE AND V2-MODE PROFISAFE-DEVICES)",2100,"TEM",1,"Simatic",0.25800000000000001,0]
["6ES71953BF030YA0","PROFIsafe-STarterkit V3.5 with PROFIsafe profile V2.6.1",2100,"TEM",1,"Simatic",0.215,0]
["6ES71957HA000XA0","SIMATIC DP, BUS UNIT FOR ET200M F. THE INTEGR.OF 1 PS A.1 IM153 FUNCTION:INSERT/REMOVE-MODULE WHILE OPERATING MODE RUN INCL. COVER FOR BUS UNIT",41.400000000000006,"TEM",1,"Simatic",0.10299999999999999,1]
["6ES71957HB000XA0","SIMATIC DP, BUS UNIT FOR ET200M F. THE INTEGR.OF TWO 40 MM WIDE I/O SUBMODULES FOR INSERT/REMOVE",92.2,"TEM",1,"Simatic",0.13200000000000001,1]
["6ES71957HC000XA0","SIMATIC DP, BUS UNIT FOR ET200M F. THE INTEGR.OF ONE 80 MM WIDE I/O SUBMODULE FOR INSERT/REMOVE",78,"TEM",1,"Simatic",0.11700000000000001,1]
["6ES71957HD100XA0","SIMATIC DP, BUS UNIT FOR ET200M FOR INTEGRATING 2 IM153-2 RED. FUNCTION: INSERT/REMOVE WHILE OPERATING MODE RUN",126,"TEM",1,"Simatic",0.128,1]
["6ES71957HG000XA0","SIMATIC S7, SEPARATOR BUS MODUL BETWEEN F- AND STANDARD MODULES USE ONLY WITH SEPARATOR MODULE",59.7,"TEM",1,"Simatic",0.11899999999999999,1]
["6ES71957KF000XA0","SIMATIC S7, SEPARATOR MODULE BETWEEN F- AND STANDARD MODULES WITH REDUNDANT ET200M INTERFACE MODULES USE ONLY WITH SEPARATOR BUS MODULE",157,"TEM",1,"Simatic",0.29499999999999998,1]
["6ES72111AE400XB0","SIMATIC S7-1200, CPU 1211C, COMPACT CPU, DC/DC/DC, ONBOARD I/O: 6 DI 24V DC; 4 DO 24 V DC; 2 AI  0 - 10V DC, POWER SUPPLY: DC 20.4 - 28.8 V DC, PROGRAM/DATA MEMORY: 50 KB",174,"TEM",1,"S7-1200",0.33700000000000002,1]
["6ES72111BE400XB0","SIMATIC S7-1200, CPU 1211C, COMPACT CPU, AC/DC/RELAY, ONBOARD I/O: 6 DI 24V DC; 4 DO RELAY 2A; 2 AI  0 - 10V DC, POWER SUPPLY: AC 85 - 264 V AC AT 47 - 63 HZ, PROGRAM/DATA MEMORY: 50 KB",174,"TEM",1,"S7-1200",0.38100000000000001,1]
["6ES72111HE400XB0","SIMATIC S7-1200, CPU 1211C, COMPACT CPU, DC/DC/RELAY, ONBOARD I/O: 6 DI 24V DC; 4 DO RELAY 2A; 2 AI  0 - 10V DC, POWER SUPPLY: DC 20.4 - 28.8 V DC, PROGRAM/DATA MEMORY: 50 KB",174,"TEM",1,"S7-1200",0.34599999999999997,1]
["6ES72121AE400XB0","SIMATIC S7-1200, CPU 1212C, COMPACT CPU, DC/DC/DC, ONBOARD I/O: 8 DI 24V DC; 6 DO 24 V DC; 2 AI  0 - 10V DC, POWER SUPPLY: DC 20.4 - 28.8 V DC, PROGRAM/DATA MEMORY: 75 KB",234,"TEM",1,"S7-1200",0.34,1]
["6ES72121AF400XB0","SIMATIC S7-1200F, CPU 1212 FC, COMPACT CPU, DC/DC/DC, ONBOARD I/O: 8 DI 24V DC; 6 DO 24 V DC; 2 AI  0 - 10V DC, POWER SUPPLY: DC 20.4 - 28.8 V DC, PROGRAM/DATA MEMORY 100 KB",342,"TEM",1,"S7-1200",0.34,1]
["6ES72121BD344YB0","SIMATIC S7-1200, STARTERKIT, CONSISTING OF: CPU 1212C AC/DC/RLY, INPUT SIMULATOR, STEP7 BASIC CD, MANUAL CD, INFO MATERIAL, SYSTAINER",587,"TEM",1,"Simatic",2.62,0]
["6ES72121BE400XB0","SIMATIC S7-1200, CPU 1212C, COMPACT CPU, AC/DC/RLY, ONBOARD I/O: 8 DI 24V DC; 6 DO RELAY 2A; 2 AI  0 - 10V DC, POWER SUPPLY: AC 85 - 264 V AC AT 47 - 63 HZ, PROGRAM/DATA MEMORY: 75 KB",234,"TEM",1,"S7-1200",0.38800000000000001,1]
["6ES72121HE400XB0","SIMATIC S7-1200, CPU 1212C, COMPACT CPU, DC/DC/RLY, ONBOARD I/O: 8 DI 24V DC; 6 DO RELAY 2A; 2 AI  0 - 10V DC, POWER SUPPLY: DC 20.4 - 28.8 V DC, PROGRAM/DATA MEMORY: 75 KB",234,"TEM",1,"S7-1200",0.35399999999999998,1]
["6ES72121HF400XB0","SIMATIC S7-1200, CPU 1212FC, COMPACT CPU, DC/DC/RLY, ONBOARD I/O: 8 DI 24V DC; 6 DO RELAY 2A; 2 AI  0 - 10V DC, POWER SUPPLY: DC 20.4 - 28.8 V DC, PROGRAM/DATA MEMORY 100 KB",342,"TEM",1,"S7-1200",0.35399999999999998,1]
["6ES72121HF404YB0","SIMATIC S7-1200, FAIL-SAFE STARTERKIT CONSISTING OF: CPU 1214 FC DC/DC/RELAY, SM 1226 F-DI 16X 24V DC, SM 1226 F-DQ 4X 24V DC, INPUT SIMULATOR, STEP7 BASIC CD, STEP7 SAFETY BASIC CD, MANUAL CD, INFO MATERIAL, SYSTAINER",1305,"TEM",1,"Simatic",3.5,0]
["6ES72121HF414YB0","SIMATIC S7-1200, FAIL-SAFE STARTERKIT CONSISTING OF: CPU 1212 FC DC/DC/RELAY, SM 1226 F-DI 16X 24V DC, SM 1226 F-DQ 4X 24V DC, INPUT SIMULATOR, STEP7 BASIC CD, STEP7 SAFETY BASIC CD, MANUAL CD, INFO MATERIAL, SYSTAINER",1060,"TEM",1,"Simatic",3.5,0]
["6ES72141AE304AB3","TRAINING BUNDLE CPU1214C DC/DC/DC, CONSISTING OF: 6 X S7-1200 CPU 1214C DC/DC/DC, 6 X STEP7 BASIC, SINGLE LIC., 6 X ANALOG OUTPUT SB1232, 1 AO, 6 X SIMULATOR MOD. SIM1274 8CH, 6 X RJ45 CABLE, LENGTH 6 M, ******************************* FOR EDUCATIONAL PURPOSES ONLY",1793,"TEM",1,"Simatic",9.5,0]
["6ES72141AF400XB0","SIMATIC S7-1200F, CPU 1214 FC, COMPACT CPU, DC/DC/DC, ONBOARD I/O: 14 DI 24V DC; 10 DO 24 V DC; 2 AI  0 - 10V DC, POWER SUPPLY: DC 20.4 - 28.8 V DC, PROGRAM/DATA MEMORY 125 KB",538,"TEM",1,"S7-1200",0.433,1]
["6ES72141AG400XB0","SIMATIC S7-1200, CPU 1214C, COMPACT CPU, DC/DC/DC, ONBOARD I/O: 14 DI 24V DC; 10 DO 24 V DC; 2 AI  0 - 10V DC, POWER SUPPLY: DC 20.4 - 28.8 V DC, PROGRAM/DATA MEMORY: 100 KB",353,"TEM",1,"S7-1200",0.41199999999999998,1]
["6ES72141BE304AB3","TRAINING BUNDLE CPU 1214C AC/DC/RLY, CONSISTING OF: 6 X S7-1200 CPU1214C AC/DC/RLY, 6 X STEP7 BASIC, SINGLE LIC., 6 X ANALOG OUTPUT SB1232, 1 AO, 6 X SIMULATOR MOD. SIM1274 8CH, 6 X RJ45 CABLE, LENGTH 6 M, ******************************* FOR EDUCATIONAL PURPOSES ONLY",1793,"TEM",1,"Simatic",9.5,0]
["6ES72141BG400XB0","SIMATIC S7-1200, CPU 1214C, COMPACT CPU, AC/DC/RLY, ONBOARD I/O: 14 DI 24V DC; 10 DO RELAY 2A; 2 AI  0 - 10V DC, POWER SUPPLY: AC 85 - 264 V AC AT 47 - 63 HZ, PROGRAM/DATA MEMORY: 100 KB",353,"TEM",1,"S7-1200",0.49099999999999999,1]
["6ES72141HF400XB0","SIMATIC S7-1200F, CPU 1214 FC, COMPACT CPU, DC/DC/RELAY, ONBOARD I/O: 14 DI 24V DC; 10 DO RELAY 2A; 2 AI  0 - 10V DC, POWER SUPPLY: DC 20.4 - 28.8 V DC, PROGRAM/DATA MEMORY 125 KB",538,"TEM",1,"S7-1200",0.45200000000000001,1]
["6ES72141HG400XB0","SIMATIC S7-1200, CPU 1214C, COMPACT CPU, DC/DC/RELAY, ONBOARD I/O: 14 DI 24V DC; 10 DO RELAY 2A; 2 AI  0 - 10V DC, POWER SUPPLY: DC 20.4 - 28.8 V DC, PROGRAM/DATA MEMORY: 100 KB",353,"TEM",1,"S7-1200",0.45200000000000001,1]
["6ES72151AF400XB0","SIMATIC S7-1200F, CPU 1215 FC, COMPACT CPU, DC/DC/DC, 2 PROFINET PORT, ONBOARD I/O: 14 DI 24VDC; 10 DO 24V DC 0.5A; 2 AI 0-10V DC, 2 AO 0-20MA DC, POWER SUPPLY: DC 20.4 - 28.8 V DC, PROGRAM/DATA MEMORY 150 KB",791,"TEM",1,"S7-1200",0.46700000000000003,1]
["6ES72151AG400XB0","SIMATIC S7-1200, CPU 1215C, COMPACT CPU, DC/DC/DC, 2 PROFINET PORT, ONBOARD I/O: 14 DI 24V DC; 10 DO 24V DC 0.5A 2 AI 0-10V DC, 2 AO 0-20MA DC, POWER SUPPLY: DC 20.4 - 28.8 V DC, PROGRAM/DATA MEMORY: 125 KB",532,"TEM",1,"S7-1200",0.44600000000000001,1]
["6ES72151AL400XB0","SIMATIC S7-1200, CPU 1215C, COMPACT CPU, DC/DC/DC, 2 PROFINET PORT, ONBOARD I/O: 14 DI 24V DC; 10 DO 24V DC 0.5A 2 AI 0-10V DC, 2 AO 0-20MA DC, POWER SUPPLY: DC 20.4 - 28.8 V DC, PROJECT SPECIFIC: 200KB MEMORY",1564,"TEM",1,"S7-1200",0.45700000000000002,1]
["6ES72151AM400XB0","SIMATIC S7-1200, CPU 1215C, COMPACT CPU, DC/DC/DC, 2 PROFINET PORT, ONBOARD I/O: 14 DI 24V DC; 10 DO 24V DC 0.5A 2 AI 0-10V DC, 2 AO 0-20MA DC, POWER SUPPLY: DC 20.4 - 28.8 V DC, PROJECT SPECIFIC: 500KB MEMORY",2688,"TEM",1,"S7-1200",0.45200000000000001,1]
["6ES72151BG400XB0","SIMATIC S7-1200, CPU 1215C, COMPACT CPU, AC/DC/RELAY, 2 PROFINET PORT, ONBOARD I/O: 14 DI 24V DC; 10 DO RELAY 2A, 2 AI 0-10V DC, 2 AO 0-20MA DC, POWER SUPPLY: AC 85 - 264 V AC AT 47 - 63 HZ, PROGRAM/DATA MEMORY: 125 KB",532,"TEM",1,"S7-1200",0.503,1]
["6ES72151HF400XB0","SIMATIC S7-1200F, CPU 1215 FC, COMPACT CPU, DC/DC/RELAY, 2 PROFINET PORT, ONBOARD I/O: 14 DI 24V DC; 10 DO RELAY 2A, 2 AI 0-10V DC, 2 AO 0-20MA DC, POWER SUPPLY: DC 20.4 - 28.8 V DC, PROGRAM/DATA MEMORY 150 KB",791,"TEM",1,"S7-1200",0.47499999999999998,1]
["6ES72151HG400XB0","SIMATIC S7-1200, CPU 1215C, COMPACT CPU, DC/DC/RELAY, 2 PROFINET PORT, ONBOARD I/O: 14 DI 24V DC; 10 DO RELAY 2A, 2 AI 0-10V DC, 2 AO 0-20MA DC, POWER SUPPLY: DC 20.4 - 28.8 V DC, PROGRAM/DATA MEMORY: 125 KB",532,"TEM",1,"S7-1200",0.47299999999999998,1]
["6ES72171AG400XB0","SIMATIC S7-1200, CPU 1217C, COMPACT CPU, DC/DC/DC, 2 PROFINET PORT ONBOARD I/O: 10 DI 24V DC; 4 DI RS422/485; 6 DO 24V DC; 0,5A; 4 DO RS422/485; 2 AI 0- 10V DC, 2 AQ 0- 20MA; POWER SUPPLY: DC 20.4 - 28.8 V DC, PROGRAM/DATA MEMORY: 150 KB",768,"TEM",1,"S7-1200",0.504,1]
["6ES72211BF320XB0","SIMATIC S7-1200, DIGITAL INPUT SM 1221, 8DI, 24V DC, SINK/SOURCE INPUT",102,"TEM",1,"S7-1200",0.17,1]
["6ES72211BH320XB0","SIMATIC S7-1200, DIGITAL INPUT SM 1221, 16 DI, 24VDC, SINK/SOURCE INPUT",162,"TEM",1,"S7-1200",0.21,1]
["6ES72213AD300XB0","SIMATIC S7-1200, DIGITAL INPUT SB 1221, 4DI, 5VDC 200KHZ, SOURCE",59.7,"TEM",1,"S7-1200",3.5000000000000003E-2,1]
["6ES72213BD300XB0","SIMATIC S7-1200, DIGITAL INPUT SB 1221, 4DI, 24VDC 200KHZ, SOURCE",59.7,"TEM",1,"S7-1200",2.7E-2,1]
["6ES72221AD300XB0","SIMATIC S7-1200, DIGITAL OUTPUT SB 1222, 4DQ, 5VDC 200KHZ",59.7,"TEM",1,"S7-1200",3.3000000000000002E-2,1]
["6ES72221BD300XB0","SIMATIC S7-1200, DIGITAL OUTPUT SB 1222, 4DQ, 24VDC 200KHZ",59.7,"TEM",1,"S7-1200",2.7E-2,1]
["6ES72221BF320XB0","SIMATIC S7-1200, DIGITAL OUTPUT SM 1222, 8 DO, 24V DC, TRANSISTOR 0.5A",102,"TEM",1,"S7-1200",0.18,1]
["6ES72221BH320XB0","SIMATIC S7-1200, DIGITAL OUTPUT SM 1222, 16 DO, 24V DC, TRANSISTOR 0.5A",162,"TEM",1,"S7-1200",0.22,1]
["6ES72221HF320XB0","SIMATIC S7-1200, DIGITAL OUTPUT SM 1222, 8 DO, RELAY 2A",102,"TEM",1,"S7-1200",0.19,1]
["6ES72221HH320XB0","SIMATIC S7-1200, DIGITAL OUTPUT SM 1222, 16 DO, RELAY 2A",162,"TEM",1,"S7-1200",0.26,1]
["6ES72221XF300XB0","SIMATIC S7-1200, DIGITAL OUTPUT SM 1222, 8 DO, RELAY CHANGEOVER CONTACT",120,"TEM",1,"S7-1200",0.372,1]
["6ES72221XF320XB0","SIMATIC S7-1200, DIGITAL OUTPUT SM 1222, 8 DO, RELAY CHANGEOVER CONTACT",120,"TEM",1,"S7-1200",0.372,1]
["6ES72230BD300XB0","SIMATIC S7-1200, DIGITAL I/O SB 1223, 2 DI / 2 DO, 2 DI 24V DC/2 DO 24V DC",59.7,"TEM",1,"S7-1200",2.9000000000000001E-2,1]
["6ES72231BH320XB0","SIMATIC S7-1200, DIGITAL I/O SM 1223, 8DI / 8DO, 8DI DC 24 V, SINK/SOURCE, 8DO, TRANSISTOR 0.5A",162,"TEM",1,"S7-1200",0.21,1]
["6ES72231BL320XB0","SIMATIC S7-1200, DIGITAL I/O SM 1223, 16DI / 16DO, 16DI DC 24 V, SINK/SOURCE, 16DO, TRANSISTOR 0.5A",257,"TEM",1,"S7-1200",0.31,1]
["6ES72231PH320XB0","SIMATIC S7-1200, DIGITAL I/O SM 1223, 8DI / 8DO, 8DI DC 24 V, SINK/SOURCE, 8DO, RELAY 2A",162,"TEM",1,"S7-1200",0.21,1]
["6ES72231PL320XB0","SIMATIC S7-1200, DIGITAL I/O SM 1223, 16DI / 16DO, 16DI DC 24 V, SINK/SOURCE, 16DO, RELAY 2A",257,"TEM",1,"S7-1200",0.23,1]
["6ES72231QH320XB0","SIMATIC S7-1200, DIGITAL I/O SM 1223, 8DI AC / 8DO RLY, 8DI 120/230 V AC, 8DO, RELAY 2A",222,"TEM",1,"S7-1200",0.21,1]
["6ES72233AD300XB0","SIMATIC S7-1200, DIGITAL I/O SB 1223, 2DI/2DQ, 5VDC 200KHZ",59.7,"TEM",1,"S7-1200",3.5999999999999997E-2,1]
["6ES72233BD300XB0","SIMATIC S7-1200, DIGITAL I/O SB 1223, 2DI/2DQ, 24VDC 200KHZ",59.7,"TEM",1,"S7-1200",3.5000000000000003E-2,1]
["6ES72266BA320XB0","SIMATIC S7-1200, DIGITAL INPUT, SM 1226, F-DI 16X 24VDC, PROFISAFE, 70 MM WIDTH, UP TO PL E (ISO 13849-1)/ UP TO SIL3 (IEC 61508)",180,"TEM",1,"S7-1200",0.09,1]
["6ES72266DA320XB0","SIMATIC S7-1200, DIGITAL OUTPUT SM 1226, F-DQ 4X 24VDC 2A, PROFISAFE, 70 MM WIDTH, UP TO PL E (ISO 13849-1)/ UP TO SIL3 (IEC 61508)",180,"TEM",1,"S7-1200",0.09,1]
["6ES72266RA320XB0","SIMATIC S7-1200, RELAY OUTPUT SM 1226, F-DQ 2X RLY 5A, PROFISAFE, 70 MM WIDTH, UP TO PL E (ISO 13849-1)/ UP TO SIL3 (IEC 61508)",248,"TEM",1,"S7-1200",1E-3,1]
["6ES72314HA300XB0","SIMATIC S7-1200, ANALOG INPUT SB 1231, 1 AI, +/- 10V DC (12 BIT RES.) OR 0 - 20 MA",59.7,"TEM",1,"S7-1200",2.7E-2,1]
["6ES72314HD320XB0","SIMATIC S7-1200, ANALOG INPUT, SM 1231, 4 AI, +/-10V, +/-5V, +/-2.5V, OR 0-20MA/4-20 MA, 12 BIT + SIGN BIT (13 BIT ADC)",209,"TEM",1,"S7-1200",0.17199999999999999,1]
["6ES72314HF320XB0","SIMATIC S7-1200, ANALOG INPUT, SM 1231, 8 AI, +/-10V, +/-5V, +/-2.5V, OR 0-20MA/4-20 MA, 12 BIT + SIGN OR (13 BIT ADC)",341,"TEM",1,"S7-1200",0.21199999999999999,1]
["6ES72315ND320XB0","SIMATIC S7-1200, ANALOG INPUT, SM 1231, 4 AI, +/-10V, +/-5V, +/-2.5V, +/-1.25 OR 0-20MA/4-20 MA, 15 BIT + SIGN BIT",341,"TEM",1,"S7-1200",0.16500000000000001,1]
["6ES72315PA300XB0","SIMATIC S7-1200, RTD INPUT, SB 1231 RTD, 1 AI RTD, 1 CHANNEL, PT 100 AND PT1000",90.100000000000009,"TEM",1,"S7-1200",3.5000000000000003E-2,1]
["6ES72315PD320XB0","SIMATIC S7-1200, ANALOG INPUT, SM 1231 RTD, 4 X  AI RTD MODULE",293,"TEM",1,"S7-1200",0.20699999999999999,1]
["6ES72315PF320XB0","SIMATIC S7-1200, ANALOG INPUT, SM 1231RTD, 8 X AI RTD MODULE,",472,"TEM",1,"S7-1200",0.29599999999999999,1]
["6ES72315QA300XB0","SIMATIC S7-1200, ANALOG SB 1231 T, 1 X AI THERMOCOUPLE, TYPE J OR K",90.100000000000009,"TEM",1,"S7-1200",3.3000000000000002E-2,1]
["6ES72315QD320XB0","SIMATIC S7-1200, ANALOG INPUT, SM 1231 TC, 4 AI THERMOCOUPLE",293,"TEM",1,"S7-1200",0.16900000000000001,1]
["6ES72315QF320XB0","SIMATIC S7-1200, ANALOG INPUT, SM 1231 TC, 8 AI THERMOCOUPLE",423,"TEM",1,"S7-1200",0.21099999999999999,1]
["6ES72324HA300XB0","SIMATIC S7-1200,  ANALOG OUTPUT SB 1232, 1 AO, +/- 10VDC (12 BIT RES.) OR 0 - 20 MA (11 BIT RES)",90.100000000000009,"TEM",1,"S7-1200",2.8000000000000001E-2,1]
["6ES72324HB320XB0","SIMATIC S7-1200, ANALOG OUTPUT, SM 1232, 2 AO, +/-10V, 14 BIT RESOLUTION, OR 0 - 20 MA/4 - 20 MA, 13 BIT RESOLUTION",222,"TEM",1,"S7-1200",0.16900000000000001,1]
["6ES72324HD320XB0","SIMATIC S7-1200, ANALOG OUTPUT, SM 1232, 4 AO, +/-10V, 14 BIT RESOLUTION, OR 0 - 20 MA/4 - 20 MA, 13 BIT RESOLUTION",353,"TEM",1,"S7-1200",0.214,1]
["6ES72344HE320XB0","SIMATIC S7-1200, ANALOG I/O SM 1234, 4 AI / 2 AO, +/-10V, 14 BIT RESOLUTION OR 0(4) - 20 MA, 13 BIT RESOLUTION",305,"TEM",1,"S7-1200",0.218,1]
["6ES72385XA320XB0","SIMATIC S7-1200, Analog input, SM 1238 Energy Meter 480V AC, Energy measurement module for recording electrical parameters in 1 and 3 phase networks (TN, TT) up to 480VAC; current range: 1A, 5A; recording of voltages, currents, phase angels, power, energy values, frequencies; channel diagnosis",273,"TEM",1,"S7-1200",0.2,1]
["6ES72411AH320XB0","SIMATIC S7-1200, COMMUNICATION MODULE CM 1241, RS232, 9 PIN SUB D (MALE), SUPPORTS MESSAGE BASED FREEPORT",120,"TEM",1,"S7-1200",0.156,1]
["6ES72411CH301XB0","SIMATIC S7-1200, COMMUNICATION COMMUNICATION BOARD CB 1241, RS485, SCREW CONNECTOR SUPPORTS MESSAGE BASED FREEPORT",77.2,"TEM",1,"S7-1200",2.9000000000000001E-2,1]
["6ES72411CH320XB0","SIMATIC S7-1200, COMMUNICATION MODULE CM 1241, RS422/485, 9 PIN SUB D (FEMALE) SUPPORTS MESSAGE BASED FREEPORT",120,"TEM",1,"S7-1200",0.159,1]
["6ES72741XA300XA0","SIMATIC S7-1200, SIM1274 ANALOG SIMULATOR 2 CH POTENTIOMETER INPUT,",51.7,"TEM",1,"S7-1200",1.2999999999999999E-2,1]
["6ES72741XF300XA0","SIMATIC S7-1200, SIMULATOR MODULE  SIM1274, 8 CHANNEL SIMULATOR DC INPUT SWITCHES",96,"TEM",1,"S7-1200",1.9E-2,1]
["6ES72741XH300XA0","SIMATIC S7-1200, SIMULATOR MODULE SIM 1274, 14 CHANNEL SIMULATOR DC INPUT SWITCHES",132,"TEM",1,"S7-1200",2.8000000000000001E-2,1]
["6ES72741XK300XA0","SIMATIC S7-1200, SIMULATOR MODULE S7-1217C, 14 CHANNEL SIMULATOR, 10X 24V DC INPUT SWITCHES, 4X 1.5V DIFFERENTIAL INPUT SWITCHES,",132,"TEM",1,"S7-1200",4.1000000000000002E-2,1]
["6ES72784BD320XB0","SIMATIC S7-1200, SM1278  IO-LINK, 4 X IO-LINK MASTER",213,"TEM",1,"S7-1200",0.19700000000000001,1]
["6ES72903AA300XA0","SIMATIC S7-1200, RJ45 STRAIN RELIEF, SINGLE PORT 4 PIECES PER PACKAGING UNIT",17.600000000000001,"ΠΑΚ",1,"S7-1200",0.03,1]
["6ES72903AB300XA0","SIMATIC S7-1200, RJ45 STRAIN RELIEF, DUAL PORT 4 PIECES PER PACKAGING UNIT",23.400000000000002,"ΠΑΚ",1,"S7-1200",0.1,1]
["6ES72906AA300XA0","SIMATIC S7-1200, EXPANSION CABLE TWO-ROW ARRANGEMENT FOR SM 12XX, 2.0 M",53.800000000000004,"TEM",1,"S7-1200",0.23699999999999999,1]
["6ES72911AA300XA0","SIMATIC S7-1200, SPARE PART DOOR KIT, CPU 1211/1212 (CPU 1211/1212 TOP & BOTTOM DOOR / SIGNAL BOARD COVER) 4 PIECES EACH",23.900000000000002,"ΠΑΚ",1,"S7-1200",0.14499999999999999,0]
["6ES72911AB300XA0","SIMATIC S7-1200, SPARE PART DOOR KIT, CPU 1214 (CPU 1214 TOP & BOTTOM DOOR / SIGNAL BOARD COVER) 4 PIECES EACH",23.900000000000002,"ΠΑΚ",1,"S7-1200",0.157,0]
["6ES72911AC300XA0","SIMATIC S7-1200, SPARE PART DOOR KIT CPU 1215C (CPU 1215C TOP & BOTTOM DOOR / SIGNAL BOARD COVER) 4 PIECES EACH",29.900000000000002,"ΠΑΚ",1,"S7-1200",0.06,0]
["6ES72911AD300XA0","SIMATIC S7-1200, SPARE PART DOOR KIT CPU 1217C (CPU 1217C TOP & BOTTOM DOOR / SIGNAL BOARD COVER) 4 PIECES EACH",29.900000000000002,"TEM",1,"S7-1200",0.17,0]
["6ES72911BA300XA0","SIMATIC S7-1200, SPARE PART DOOR KIT, SIGNAL MODULE 45MM, (SINGAL MODULE 45MM  TOP & BOTTOM DOOR) 6 PIECES EACH",17.900000000000002,"ΠΑΚ",1,"S7-1200",8.4000000000000005E-2,0]
["6ES72911BB300XA0","SIMATIC S7-1200, SPARE PART DOOR KIT, SIGNAL MODULE 70MM, (SINGAL MODULE 70MM TOP & BOTTOM DOOR) 6 PIECES EACH",17.900000000000002,"ΠΑΚ",1,"S7-1200",0.11,0]
["6ES72911CC300XA0","SIMATIC S7-1200, SPARE PART DOOR KIT, COMMUNICATION MODULES (COMMUNICATION MODULE TOP & BOTTOM DOOR) 4 PIECES EACH",17.900000000000002,"ΠΑΚ",1,"S7-1200",6.7000000000000004E-2,0]
["6ES72921AG300XA0","SIMATIC S7-1200, SPARE PART I/O TERMINAL BLOCK TIN DIGITAL SIGNAL MODULE 8CH/16CH (4 PIECES W. 7 SCREWS EACH)",23.900000000000002,"ΠΑΚ",1,"S7-1200",7.9000000000000001E-2,1]
["6ES72921AG400XA0","SIMATIC S7-1200, SPARE PART I/O TERMINAL BLOCK TIN, KEYED, FOR DIGITAL SIGNAL MODULES 8CH/16CH (4 PIECES W. 7 SCREWS EACH)",23.900000000000002,"ΠΑΚ",1,"S7-1200",7.9000000000000001E-2,1]
["6ES72921AG400XA1","SIMATIC S7-1200, SPARE PART, I/O TERMINAL BLOCK TIN, KEYED LEFT, FOR DIGITAL SIGNAL MODULES 8CH/16CH (4 PIECES W. 7 SCREWS EACH)",23.900000000000002,"ΠΑΚ",1,"S7-1200",7.9000000000000001E-2,1]
["6ES72921AG400XA2","SIMATIC S7-1200, Spare part, I/O Terminal block TIN, keyed middle, Top, 7 pins for Voltage Input SM 1238 Energy Meter (4 pieces w. 7 screws each)",23.5,"TEM",1,"S7-1200",0.08,1]
["6ES72921AH300XA0","SIMATIC S7-1200, SPARE PART I/O TERMINAL BLOCK TIN CPU1211C/1212C BOTTOM CONNECTOR (4 PIECES W. 8 SCREWS EACH)",35.9,"ΠΑΚ",1,"S7-1200",8.8999999999999996E-2,1]
["6ES72921AH400XA0","SIMATIC S7-1200, SPARE PART, I/O TERMINAL BLOCK TIN, KEYED RIGHT, CPU1211C/1212C BOTTOM CONNECTOR (4 PIECES W. 8 SCREWS EACH)",35.9,"ΠΑΚ",1,"S7-1200",8.8999999999999996E-2,1]
["6ES72921AK300XA0","SIMATIC S7-1200, SPARE PART I/O TERMINAL BLOCK TIN CPU 1217C TOP CONNECTOR (4 PIECES W. 10 SCREWS EACH)",48,"ΠΑΚ",1,"S7-1200",7.9000000000000001E-2,1]
["6ES72921AL300XA0","SIMATIC S7-1200, SPARE PART I/O TERMINAL BLOCK TIN DIGITAL SIGNAL MODUL 32CH (4 PIECES W. 11 SCREWS EACH)",35.9,"ΠΑΚ",1,"S7-1200",0.105,1]
["6ES72921AL400XA0","SIMATIC S7-1200, SPARE PART, I/O TERMINAL BLOCK TIN, KEYED RIGHT, DIGITAL SIGNAL MODUL 32CH, (4 PIECES W. 11 SCREWS EACH)",35.9,"ΠΑΚ",1,"S7-1200",0.105,1]
["6ES72921AM300XA0","SIMATIC S7-1200, SPARE PART I/O TERMINAL BLOCK TIN CPU1214C/1215C BOTTOM CONNECTOR (4 PIECES W. 12 SCREWS EACH)",35.9,"ΠΑΚ",1,"S7-1200",0.115,1]
["6ES72921AM400XA0","SIMATIC S7-1200, SPARE PART, I/O TERMINAL BLOCK TIN, KEYED RIGHT, CPU1214C/1215C BOTTOM CONNECTOR (4 PIECES W. 12 SCREWS EACH)",35.9,"ΠΑΚ",1,"S7-1200",9.1999999999999998E-2,1]
["6ES72921AP300XA0","SIMATIC S7-1200, SPARE PART I/O TERMINAL BLOCK TIN CPU 1211C / 1212C TOP CONNECTOR (4 PIECES W. 14 SCREWS EACH)",48,"ΠΑΚ",1,"S7-1200",0.125,1]
["6ES72921AP400XA0","SIMATIC S7-1200, SPARE PART, I/O TERMINAL BLOCK TIN, KEYED RIGHT, CPU1211C/1212C TOP CONNECTOR, (4 PIECES W. 14 SCREWS EACH)",48,"ΠΑΚ",1,"S7-1200",0.125,1]
["6ES72921AR300XA0","SIMATIC S7-1200, SPARE PART I/O TERMINAL BLOCK TIN CPU 1217C TOP CONNECTOR (4 PIECES W. 16 SCREWS EACH)",48,"ΠΑΚ",1,"S7-1200",0.11600000000000001,1]
["6ES72921AT300XA0","SIMATIC S7-1200, SPARE PART I/O TERMINAL BLOCK TIN CPU 1217C BOTTOM CONNECTOR (4 PIECES W. 18SCREWS EACH)",48,"ΠΑΚ",1,"S7-1200",0.127,1]
["6ES72921AV300XA0","SIMATIC S7-1200, SPARE PART I/O TERMINAL BLOCK TIN CPU 1214C/1215C TOP CONNECTOR (4 PIECES W: 20 SCREWS EACH)",52.800000000000004,"ΠΑΚ",1,"S7-1200",0.16400000000000001,1]
["6ES72921AV400XA0","SIMATIC S7-1200, SPARE PART, I/O TERMINAL BLOCK TIN, KEYED RIGHT, CPU 1214C/1215C TOP CONNECTOR, (4 PIECES W. 20 SCREWS EACH)",52.800000000000004,"ΠΑΚ",1,"S7-1200",0.14299999999999999,1]
["6ES72921BC300XA0","SIMATIC S7-1200, SPARE PART I/O TERMINAL BLOCK GOLD ANALOG INPUTS CPU 1211C/1212C/1214C (4 PIECES W. 3 SCREWS EACH)",23.900000000000002,"ΠΑΚ",1,"S7-1200",5.6000000000000001E-2,1]
["6ES72921BF300XA0","SIMATIC S7-1200, SPARE PART I/O TERMINAL BLOCK GOLD SIGNAL BOARD (4 PIECES W. 6 SCREWS EACH)",23.900000000000002,"ΠΑΚ",1,"S7-1200",0.05,1]
["6ES72921BF300XB0","SIMATIC S7-1200, SPARE PART I/O TERMINAL BLOCK GOLD ANALOG SIGNALS CPU 1215C/1217C, (4 PIECES W. 6 SCREWS EACH)",29.900000000000002,"ΠΑΚ",1,"S7-1200",7.1999999999999995E-2,1]
["6ES72921BG300XA0","SIMATIC S7-1200, SPARE PART I/O TERMINAL BLOCK GOLD ANALOG SIGNAL MODULE 8CH/16CH (4 PIECES W. 7 SCREWS EACH)",35.9,"ΠΑΚ",1,"S7-1200",0.08,1]
["6ES72921BL300XA0","SIMATIC S7-1200, SPARE PART I/O TERMINAL BLOCK GOLD ANALOG SIGNAL MODULE 32CH (4 PIECES W. 11 SCREWS EACH)",35.9,"ΠΑΚ",1,"S7-1200",0.11,1]
["6ES72970AX300XA0","SIMATIC S7-1200, BATTERY BOARD BB 1297 FOR LONG-TERM BACKUP OF THE REALTIME CLOCK; PLUGGABLE IN THE SIGNAL BOARD S7-12XX CPU (FW3.0 AND LATER); BATTERY (CR1025) NOT INCLUDED",53.800000000000004,"TEM",1,"S7-1200",2.1000000000000001E-2,1]
["6ES72980AA400AA0","SIMATIC S7-200,TRAINING PACKAGE CONSISTING OF: 5 CPU222 DC, 5 USB/PPI-CABLE, 5 STEP7 MICRO/WIN 6 LANGUAGES (G,E,F,I,S,C), EXECUTABLE UNDER WIN2000/XP, REFERENCE-HW:SIMATIC S7-200 FOR EDUCATIONAL PURPOSES ONLY OFFER LIMITED UNTIL 12-31-2015",1251,"TEM",1,"Simatic",4,0]
["6ES73121AE140AB0","SIMATIC S7-300, CPU 312 CPU WITH MPI INTERFACE, INTEGRATED 24 V DC POWER SUPPLY 32 KBYTE WORKING MEMORY, MICRO MEMORY CARD NECESSARY",351,"TEM",1,"Simatic",0.30599999999999999,1]
["6ES73125BF040AB0","SIMATIC S7-300, CPU 312C COMPACT CPU WITH MPI, 10 DI/6 DO, 2 FAST COUNTERS (10 KHZ), INTEGRATED 24V DC POWER SUPPLY, 64 KBYTE WORKING MEMORY, FRONT CONNECTOR (1 X 40PIN) AND MICRO MEMORY CARD REQUIRED",455,"TEM",1,"Simatic",0.45800000000000002,1]
["6ES73135BG040AB0","SIMATIC S7-300, CPU 313C, COMPACT CPU WITH MPI, 24 DI/16 DO, 4AI, 2AO 1 PT100, 3 FAST COUNTERS (30 KHZ), INTEGRATED 24V DC POWER SUPPLY, 128 KBYTE WORKING MEMORY, FRONT CONNECTOR (2 X 40PIN) AND MICRO MEMORY CARD REQUIRED",936,"TEM",1,"Simatic",0.71599999999999997,1]
["6ES73136BG040AB0","SIMATIC S7-300, CPU 313C-2 PTP COMPACT CPU WITH MPI, 16 DI/16 DO, 3 FAST COUNTERS (30 KHZ), INTEGRATED INTERFACE RS485, INTEGRATED 24V DC POWER SUPPLY, 128 KBYTE WORKING MEMORY, FRONT CONNECTOR (1 X 40PIN) AND MICRO MEMORY CARD REQUIRED",999,"TEM",1,"Simatic",0.54200000000000004,1]
["6ES73136CG040AB0","SIMATIC S7-300, CPU 313C-2DP COMPACT CPU WITH MPI, 16 DI/16 DO, 3 FAST COUNTERS (30 KHZ), INTEGRATED DP INTERFACE, INTEGRATED 24V DC POWER SUPPLY, 128 KBYTE WORKING MEMORY, FRONT CONNECTOR (1 X 40PIN) AND MICRO MEMORY CARD REQUIRED",1196,"TEM",1,"Simatic",0.53700000000000003,1]
["6ES73141AG140AB0","SIMATIC S7-300, CPU 314 CPU WITH MPI INTERFACE, INTEGRATED 24V DC POWER SUPPLY, 128 KBYTE WORKING MEMORY, MICRO MEMORY CARD NECESSARY",626,"TEM",1,"Simatic",0.314,1]
["6ES73146BH040AB0","SIMATIC S7-300, CPU 314C-2 PTP COMPACT CPU WITH MPI, 24 DI/16 DO, 4AI, 2AO, 1 PT100, 4 FAST COUNTERS (60 KHZ), INTEGRATED INTERFACE RS485, INTEGRATED 24V DC POWER SUPPLY, 192 KBYTE WORKING MEMORY, FRONT CONNECTOR (2 X 40PIN) AND MICRO MEMORY CARD REQUIRED",1520,"TEM",1,"Simatic",0.73699999999999999,1]
["6ES73146CH040AB0","SIMATIC S7-300, CPU 314C-2 DP COMPACT CPU WITH MPI, 24 DI/16 DO, 4AI, 2AO, 1 PT100, 4 FAST COUNTERS (60 KHZ), INTEGRATED DP INTERFACE, INTEGRATED 24V DC POWER SUPPLY, 192 KBYTE WORKING MEMORY, FRONT CONNECTOR (2 X 40PIN) AND MICRO MEMORY CARD REQUIRED",1719,"TEM",1,"Simatic",0.73299999999999998,1]
["6ES73146EH040AB0","SIMATIC S7-300, CPU 314C-2PN/DP COMPACT CPU WITH 192 KBYTE WORKING MEMORY, 24 DI/16 DO, 4AI, 2AO, 1 PT100, 4 FAST COUNTERS (60 KHZ), 1. INTERFACE MPI/DP 12MBIT/S, 2. INTERFACE ETHERNET PROFINET, WITH 2 PORT SWITCH, INTEGRATED 24V DC POWER SUPPLY, FRONT CONNECTOR (2 X 40PIN) AND MICRO MEMORY CARD REQUIRED",1868,"TEM",1,"Simatic",0.80200000000000005,1]
["6ES73146EH044AB3","TRAINING BUNDLE CPU 314C-2 PN/DP; CONSISTING OF: S7-300 CPU 314C-2 PN/DP 192 KB, POWER SUPPLY PS 307 24V/5A, SIMULATOR MODULE SM 374, RAIL 480MM, MICRO MEMORY CARD 512 KBYTE, PC-ADAPTER USB, 2 X 40-PIN FRONT CONNECTOR ******************************* FOR EDUCATIONAL PURPOSES ONLY",1628,"TEM",1,"Simatic",3.5,0]
["6ES73146EH044AB4","UPGRADE TRAINING BUNDLE CPU 314C-2 PN/DP; CONSISTING OF: S7-300 CPU 314C-2 PN/DP 192 KB, SM323, 16DI/DO, DC24V, 0,5A, MICRO MEMORY CARD 512 KBYTE, 3 X 40-PIN FRONT CONNECTOR ETHERNET CORD RJ45/RJ45 6M, ******************************* FOR EDUCATIONAL PURPOSES ONLY",812,"TEM",1,"Simatic",1.8,0]
["6ES73146EH044AB8","OEM EXAMINATION BUNDLE CPU 314C-2 PN/DP, CONSISTING OF: S7-300 CPU 314C-2 PN/DP 192 KB, SM322, 8DA, DC24V, 2A, MICRO MEMORY CARD 512 KBYTE, 2 X 40-PIN FRONT CONNECTOR, 1 X 20-PIN FRONT CONNECTOR, S7-300 RAIL L=480MM, ETHERNET CORD RJ45/RJ45 6M, SOFTWARE FOR TRAINING V13 SP1 ******************************* FOR EDUCATIONAL PURPOSES ONLY OFFER LIMITED UNTIL 01-13-2017",714,"TEM",1,"Simatic",3.2,0]
["6ES73152AH140AB0","SIMATIC S7-300, CPU 315-2DP CPU WITH MPI INTERFACE INTEGRATED 24 V DC POWER SUPPLY 256 KBYTE WORKING MEMORY 2. INTERFACE DP-MASTER/SLAVE MICRO MEMORY CARD NECESSARY",1564,"TEM",1,"Simatic",0.33200000000000002,1]
["6ES73152EH140AB0","SIMATIC S7-300 CPU 315-2 PN/DP, CENTRAL PROCESSING UNIT WITH 384 KBYTE WORKING MEMORY, 1. INTERFACE MPI/DP 12MBIT/S, 2. INTERFACE ETHERNET PROFINET, WITH 2 PORT SWITCH, MICRO MEMORY CARD NECESSARY",2209,"TEM",1,"Simatic",0.38500000000000001,1]
["6ES73152FH144AB1","TRAINING BUNDLE CPU315-2PN CONTAINS S7-300 CPU 315F-PN POWER SUPPLY PS 307 5A, 1 X SM323 16DI/16DO, 1 X SM334 4AI/ 2AO, DIN RAIL 480MM MICRO MEMORY CARD 512 KBYTE, S7 DISTRIBUTED SAFETY V5.4 ******************************* FOR EDUCATIONAL PURPOSES ONLY",2853,"TEM",1,"Simatic",2.6,0]
["6ES73152FJ140AB0","SIMATIC S7-300 CPU315F-2 PN/DP, CENTRAL PROCESSING UNIT WITH 512 KBYTE WORKING MEMORY, 1. INTERFACE MPI/DP 12MBIT/S, 2. INTERFACE ETHERNET PROFINET, WITH 2 PORT SWITCH, MICRO MEMORY CARD NECESSARY",2624,"TEM",1,"Simatic",0.38800000000000001,1]
["6ES73156FF040AB0","SIMATIC S7-300, CPU 315F-2DP FAILSAFE CPU WITH MPI INTERFACE INTEGRATED 24V DC POWER SUPPLY, 384 KB WORKING MEMORY, 40MM WIDE, 2. INTERFACE DP-MASTER/SLAVE MICRO MEMORY CARD REQUIRED",1895,"TEM",1,"Simatic",0.33900000000000002,1]
["6ES73157TJ100AB0","SIMATIC S7-300, CPU 315T-3 PN/DP, CENTRAL PROCESSING UNIT FOR PLC AND TECHNOLOGY, 384 KBYTE WORKING MEMORY, 1. INTERFACE MPI/DP 12MBIT/S, 2. INTERFACE DP(DRIVE), 3. INTERFACE ETHERNET PROFINET WITH 2 PORT SWITCH, INTEGRATED I/O FOR TECHNOLOGY, FRONT CONNECTOR (1 X 40PIN) AND MICRO MEMORY CARD MIN. 8 MB NECESSARY",2887,"TEM",1,"Simatic",0.71899999999999997,1]
["6ES73157TJ100AB1","TRAINING BUNDLE CPU315T-3 PN/DP CONSISTING OF: 1 X S7-300 CPU 315T-3 PN/DP; 1 X POWER SUPPLY PS 307 5A, 1 X IM174, 1 X SM323 16DI/16DO, 1X CONNECTION CABLE 830-2  PB, 1 X MICRO MEMORY CARD 8MB, 1 X ETHERNET CABLE RJ45/RJ45 6M 1 X DIN RAIL 480MM, 3 X FRONT CONN.,40PIN, SCREW, 1X S7-TECHNOLOGY OPTION PACKAGE ******************************* FOR EDUCATIONAL PURPOSES ONLY",2200,"TEM",1,"Simatic",4.8499999999999996,0]
["6ES73172AK140AB0","SIMATIC S7-300, CPU317-2 DP, CENTRAL PROCESSING UNIT WITH 1 MBYTE WORKING MEMORY, 1. INTERFACE MPI/DP 12MBIT/S, 2. INTERFACE DP-MASTER/SLAVE, MICRO MEMORY CARD NECESSARY",3436,"TEM",1,"Simatic",0.40400000000000003,1]
["6ES73172EK140AB0","SIMATIC S7-300 CPU 317-2 PN/DP, CENTRAL PROCESSING UNIT WITH 1 MB WORKING MEMORY, 1. INTERFACE MPI/DP 12MBIT/S, 2. INTERFACE ETHERNET PROFINET, WITH 2 PORT SWITCH, MICRO MEMORY CARD NECESSARY",3903,"TEM",1,"Simatic",0.38400000000000001,1]
["6ES73172FK140AB0","SIMATIC S7-300 CPU317F-2 PN/DP, CENTRAL PROCESSING UNIT WITH 1.5 MBYTE WORKING MEMORY, 1. INTERFACE MPI/DP 12MBIT/S, 2. INTERFACE ETHERNET PROFINET, WITH 2 PORT SWITCH, MICRO MEMORY CARD NECESSARY",4402,"TEM",1,"Simatic",0.38500000000000001,1]
["6ES73176FF040AB0","SIMATIC S7-300, CPU 317F-2DP, CENTRAL PROCESSING UNIT WITH 1.5 MBYTE WORKING MEMORY, 1. INTERFACE MPI/DP 12MBIT/S, 2. INTERFACE DP-MASTER/SLAVE, MICRO MEMORY CARD NECESSARY FOR USE WITH SOFTWARE OPTION S7 DISTRIBUTED SAFETY V5.2 SP1 AND HIGHER",4018,"TEM",1,"Simatic",0.41699999999999998,1]
["6ES73177TK100AB0","SIMATIC S7-300, CPU 317T-3 PN/DP, CENTRAL PROCESSING UNIT FOR PLC AND TECHNOLOGY, 1024 KBYTE WORKING MEMORY, 1. INTERFACE MPI/DP 12MBIT/S, 2. INTERFACE DP(DRIVE), 3. INTERFACE ETHERNET PROFINET WITH 2 PORT SWITCH, INTEGRATED I/O FOR TECHNOLOGY, FRONT CONNECTOR (1 X 40PIN) AND MICRO MEMORY CARD MIN. 8 MB NECESSARY",4877,"TEM",1,"Simatic",0.72899999999999998,1]
["6ES73177UL100AB0","SIMATIC S7-300, CPU 317TF-3 PN/DP, CENTRAL PROCESSING UNIT FOR PLC, TECHNOLOGY AND SAFETY, 1,5 MBYTE WORKING MEMORY, 1. INTERFACE MPI/DP 12MBIT/S, 2. INTERFACE DP(DRIVE), 3. INTERFACE ETHERNET PROFINET WITH 2 PORT SWITCH, INTEGRATED I/O FOR TECHNOLOGY, FRONT CONNECTOR (1 X 40PIN) AND MICRO MEMORY CARD MIN. 8 MB NECESSARY",5453,"TEM",1,"Simatic",0.73899999999999999,1]
["6ES73183EL010AB0","SIMATIC S7-300 CPU 319-3 PN/DP, CENTRAL PROCESSING UNIT WITH 2 MBYTE WORKING MEMORY, 1. INTERFACE MPI/DP 12MBIT/S, 2. INTERFACE DP-MASTER/SLAVE, 3. INTERFACE ETHERNET PROFINET, WITH 2 PORT SWITCH, MICRO MEMORY CARD NECESSARY",4693,"TEM",1,"Simatic",1.4059999999999999,1]
["6ES73183FL010AB0","SIMATIC S7-300 CPU319F-3 PN/DP, CENTRAL PROCESSING UNIT WITH 2.5 MBYTE WORKING MEMORY, 1. INTERFACE MPI/DP 12MBIT/S, 2. INTERFACE DP-MASTER/SLAVE, 3. INTERFACE ETHERNET PROFINET, WITH 2 PORT SWITCH, MICRO MEMORY CARD NECESSARY",5284,"TEM",1,"Simatic",1.407,1]
["6ES73211BH020AA0","SIMATIC S7-300, DIGITAL INPUT SM 321, OPTICALLY ISOLATED, 16DI, 24 V DC, 1 X 20 PIN",168,"TEM",1,"Simatic",0.23400000000000001,1]
["6ES73211BH100AA0","SIMATIC S7-300, DIGITAL INPUT SM 321, GALVANICALLY ISOLATED, 16DI, 24 V DC, 1 X 20 PIN, 0.05 MS INPUT DELAY",212,"TEM",1,"Simatic",0.23499999999999999,1]
["6ES73211BH500AA0","SIMATIC S7-300, DIGITAL INPUT SM 321, OPTICALLY ISOLATED 16DI, 24 V DC, SOURCE INPUT, 1 X 20 PIN",150,"TEM",1,"Simatic",0.23300000000000001,1]
["6ES73211BL000AA0","SIMATIC S7-300, DIGITAL INPUT SM 321, OPTICALLY ISOLATED 32DI, 24 V DC, 1 X 40 PIN",338,"TEM",1,"Simatic",0.30099999999999999,1]
["6ES73211BP000AA0","SIMATIC S7-300 DIGITAL INPUT SM321, OPTICALLY ISOLATED IN GROUPS OF 16, 64 DI,DC 24V, 3MS, SINKING/SOURCING TERMINAL BLOCKS 6ES7392-1.N00-0AA0 AND CABLES 6ES7392-4...0-0AA0 NECESSARY",504,"TEM",1,"Simatic",0.28599999999999998,1]
["6ES73211CH000AA0","SIMATIC S7-300, DIGITAL INPUT SM 321, OPTICALLY ISOLATED, 16 DI, AC/DC 24 - 48V WITH ONE CHANNEL PER COMMON, 1 X 40 PIN",298,"TEM",1,"Simatic",0.30599999999999999,1]
["6ES73211CH200AA0","SIMATIC S7-300, DIGITAL INPUT SM 321, OPTICALLY ISOLATED, 16 DI, DC 48-125V, 1 X 20 PIN",329,"TEM",1,"Simatic",0.25,1]
["6ES73211EL000AA0","SIMATIC S7-300, DIGITAL INPUT SM 321, OPTICALLY ISOLATED, 32 DI, 120V AC, 1 X 40 PIN",430,"TEM",1,"Simatic",0.33800000000000002,1]
["6ES73211FF010AA0","SIMATIC S7-300, DIGITAL INPUT SM 321, OPTICALLY ISOLATED, 8 DI, 120V/230V AC, 1 X 20 PIN",130,"TEM",1,"Simatic",0.254,1]
["6ES73211FF100AA0","SIMATIC S7-300, DIGITAL INPUT SM 321, OPTICALLY ISOLATED, 8 DI, 120V/230V AC, 1 X 40 PIN, WITH 1 POINT PER COMMON",190,"TEM",1,"Simatic",0.31900000000000001,1]
["6ES73211FH000AA0","SIMATIC S7-300, DIGITAL INPUT SM 321, OPTICALLY ISOLATED 16 DI, 120/230V AC, 1 X 20 PIN",217,"TEM",1,"Simatic",0.29099999999999998,1]
["6ES73217BH010AB0","SIMATIC S7-300, DIGITAL INPUT SM 321, GALVANICALLY ISOLATED, 16 DI, DC 24V, 1 X 20 PIN, PROCESS INTERRUPT, DIAGNOSTICS, FIT FOR ISOCHRONE MODE",336,"TEM",1,"Simatic",0.245,1]
["6ES73221BF010AA0","SIMATIC S7-300, DIGITAL OUTPUT SM 322, OPTICALLY ISOLATED, 8 DO, 24V DC, 2A, 1 X 20 PIN",188,"TEM",1,"Simatic",0.23400000000000001,1]
["6ES73221BH010AA0","SIMATIC S7-300, DIGITAL OUTPUT SM 322, OPTICALLY ISOLATED, 16 DO, 24V DC, 0.5A, 1 X 20 PIN SUM OF OUTPUT CURRENTS 4A/GROUP (8A/MODULE)",233,"TEM",1,"Simatic",0.24,1]
["6ES73221BH100AA0","SIMATIC S7-300, DIGITAL OUTPUT SM 322 HIGH SPEED, GALVANICALLY ISOLATED, 16 DO, 24V DC, 0.5A, 1 X 20 PIN",282,"TEM",1,"Simatic",0.246,1]
["6ES73221BL000AA0","SIMATIC S7-300, DIGITAL OUTPUT SM 322, OPTICALLY ISOLATED, 32DO, 24V DC, 0.5A, 1 X 40 PIN, SUM OF OUTPUT CURRENTS 4A/GROUP (16A/MODULE)",467,"TEM",1,"Simatic",0.30199999999999999,1]
["6ES73221BP000AA0","SIMATIC S7-300 DIGITAL OUTPUT SM322, OPTICALLY ISOLATED IN GROUPS OF 16, 64 DO, DC 24V, 0.3A, (SOURCING) TOTAL CURRENT 2A/GROUP 8A/MODULE TERMINAL BLOCKS 6ES7392-1.N00-0AA0 AND CABLES 6ES7392-4...0-0AA0 NECESSARY",704,"TEM",1,"Simatic",0.30499999999999999,1]
["6ES73221BP500AA0","SIMATIC S7-300 DIGITAL OUTPUT SM322, OPTICALLY ISOLATED IN GROUPS OF 16, 64DO, DC 24V, 0.3A M-WRITE TOTAL CURRENT 2A/GROUP 8A/MODULE TERMINAL BLOCKS 6ES7392-1.N00-0AA0 AND CABLES 6ES7392-4...0-0AA0 NECESSARY",704,"TEM",1,"Simatic",0.29699999999999999,1]
["6ES73221CF000AA0","SIMATIC S7-300, DIGITAL OUTPUT SM 322, OPTICALLY ISOLATED, 8 DO, DC 48-125V, 1.5A, 1 X 20 PIN",361,"TEM",1,"Simatic",0.31,1]
["6ES73221FF010AA0","SIMATIC S7-300, DIGITAL OUTPUT SM 322, OPTICALLY ISOLATED, 8 DO, 120/230V AC, 1A, 1 X 20 PIN",245,"TEM",1,"Simatic",0.29399999999999998,1]
["6ES73221FH000AA0","SIMATIC S7-300, DIGITAL OUTPUT SM 322, OPTICALLY ISOLATED 16 DO, 120/230V AC, 1 A, 1 X 20 PIN",355,"TEM",1,"Simatic",0.32600000000000001,1]
["6ES73221FL000AA0","SIMATIC S7-300, DIGITAL OUTPUT SM 322, OPTICALLY ISOLATED, 32 DO, AC 120V/230V, 1A, DOUBLE WIDTH HOUSING, 2 X 20 PIN",712,"TEM",1,"Simatic",0.57399999999999995,1]
["6ES73221HF010AA0","SIMATIC S7-300, DIGITAL OUTPUT SM 322, OPTICALLY ISOLATED, 8 DO (RELAY), 1 X 20 PIN, 24V DC, 2A OR 230V AC, 2A",163,"TEM",1,"Simatic",0.31,1]
["6ES73221HF100AA0","SIMATIC S7-300, DIGITAL OUTPUT SM 322, OPTICALLY ISOLATED, 8 DO (RELAY), 1 X 40 PIN, 24V DC, 5A OR 230V AC, 5A, CONNECTOR W.SPRING TERMINAL CAN BE USED FROM 6ES7392-1BM01-0AA0",199,"TEM",1,"Simatic",0.36899999999999999,1]
["6ES73221HH010AA0","SIMATIC S7-300, DIGITAL OUTPUT SM 322, OPTICALLY ISOLATED 16DO, RELAY CONTACTS, 1 X 20 PIN",347,"TEM",1,"Simatic",0.27,1]
["6ES73225FF000AB0","SIMATIC S7-300, DIGITAL OUTPUT SM 322, OPTICALLY ISOLATED, 8 DO, 120/230V AC, 2A, WITH 1 POINT PER COMMON AND SELECTABLE FAIL MODE, 1 X 40 PIN",298,"TEM",1,"Simatic",0.32,1]
["6ES73225GH000AB0","SIMATIC S7-300, DIGITAL OUTPUT SM 322, OPTICALLY ISOLATED, 16 DA (SOLID STATE RELAY), AC/DC 24 - 48V; 0.5A; 1.5A SURGE CURRENT, ONE CHANNEL PER COMMON, 1 X 40 PIN",538,"TEM",1,"Simatic",0.315,1]
["6ES73225HF000AB0","SIMATIC S7-300, DIGITAL OUTPUT SM 322, OPTICALLY ISOLATED, 8 DO (RELAY), 1 X 40 PIN, 24V DC, 120 - 230V AC, 5A WITH INTEGR. SNUBBER F. IND. LOADS",222,"TEM",1,"Simatic",0.35299999999999998,1]
["6ES73228BF000AB0","SIMATIC S7-300, DIGITAL OUTPUT SM 322, OPTICALLY ISOLATED, 8 DO, 24V DC, 0.5 A (1 X 8 DO), SHORT-CIRCUIT PROTECTION, DIAGNOSTICS, 1 X 20 PIN",391,"TEM",1,"Simatic",0.24399999999999999,1]
["6ES73231BH010AA0","SIMATIC S7-300, DIGITAL MODULE SM 323, OPTICALLY ISOLATED, 8 DI AND 8 DO, 24V DC, 0.5A AGGREGATE CURRENT 2A, 1X20 PIN",256,"TEM",1,"Simatic",0.23799999999999999,1]
["6ES73231BL000AA0","SIMATIC S7-300, DIGITAL MODULE SM 323, OPTICALLY ISOLATED, 16 DI AND 16 DO, 24V DC, 0.5A, AGGREGATE CURRENT 4A, 1X40 PIN",436,"TEM",1,"Simatic",0.30499999999999999,1]
["6ES73261BK020AB0","SIMATIC S7, DIGITAL INPUT SM 326, F-DI 24 X DC 24V, FAILSAFE DIGITAL INPUTS FOR SIMATIC S7 FAILSAFE SYSTEMS WITH DIAGNOST. INTERRUPT, UP TO CATEGORY 4 (EN954-1)/ SIL3 (IEC61508)/PLE (ISO13849), 1 X 40 PIN",949,"TEM",1,"Simatic",0.49099999999999999,1]
["6ES73261RF010AB0","SIMATIC S7, DIGITAL INPUT SM 326, 8 DI; DC 24V, NAMUR, FAILSAFE NAMUR INPUTS FOR SIMATIC S7 F SYSTEMS, UP TO CATEGORY 4 (EN954-1)/ SIL3 (IEC61508)/PLE (ISO13849), 1 X 40 PIN",914,"TEM",1,"Simatic",0.56200000000000006,1]
["6ES73262BF100AB0","SIMATIC S7, DIGITAL OUTPUT SM326, F-DO10 X DC24V/2A PP, FAILSAFE DIGITAL OUTPUTS FOR SIMATIC S7F SYSTEMS WITH DIAGNOST. INTERRUPT, LVV, UP TO CATEGORY 4 (EN954-1)/ SIL3 (IEC61508)/PLE (ISO13849), 1 X 40 PIN",1042,"TEM",1,"Simatic",0.36,1]
["6ES73262BF410AB0","SIMATIC S7, DIGITAL OUTPUT SM 326, F-DO 8 X DC 24V/2A PM FAILSAFE DIGITAL OUTPUTS P-M SWITCHING UP TO CATEGORY 4 (EN954-1)/ SIL3 (IEC61508)/PLE (ISO13849), 1 X 40 PIN",878,"TEM",1,"Simatic",0.501,1]
["6ES73262FS004AB1","TRAINING BUNDLE FAILSAFE S7-300 CONTAINS: 1 X SM326 24 F-DI 24V 1 X SM326 8 F-DO 24V/2A 1 X SEPERATOR MODUL ******************************* FOR EDUCATIONAL PURPOSES ONLY ******************************* OPTION FOR 6ES7315-2FH14-4AB1",1628,"TEM",1,"Simatic",1.6,0]
["6ES73271BH000AB0","SIMATIC S7-300, DIGITAL MODULE SM 327, OPTICALLY ISOLATED, 8 DI AND 8 DX, 24V DC, 0.5A 1 X 20 PIN, 8DX CHANNELWISE PROGRAMMABLE AS DI OR DO",293,"TEM",1,"Simatic",0.24,1]
["6ES73280AA007AA0","SIMATIC S7-300, FRONT DOOR EXTENDED FOR 32-CHANNELSIGNAL MODULES, ALLOWS CONNECTION OF 1.3 QMM OR 16 AWG WIRE SIZE ON A 32 POINT MODULE 5 PIECES PER PACKAGING UNIT",51.800000000000004,"ΠΑΚ",1,"Simatic",0.317,1]
["6ES73287AA100AA0","SIMATIC S7-300, EXTENDED FRONT DOOR  FOR SAFETY MODULES, ALLOWS CONNECTION OF 1.3 QMM OR 16 AWG WIRE SIZE 5 PIECES PER PACKAGING UNIT INCL. LABELING SHEETS AND WIRING DIAGRAM (YELLOW)",51.800000000000004,"ΠΑΚ",1,"Simatic",0.20599999999999999,1]
["6ES73287AA200AA0","SIMATIC S7-300, EXTENDED FRONT DOOR FOR COMPACT-CPU, ALLOWS CONNECTION OF 1.3 QMM OR 16 AWG WIRE SIZE 5 PIECES PER PACKAGING UNIT INCL. LABELING SHEETS AND WIRING DIAGRAM (PETROLE)",51.800000000000004,"ΠΑΚ",1,"Simatic",0.17,1]
["6ES73311KF020AB0","SIMATIC S7-300, ANALOG INPUT SM 331, OPTICALLY ISOLATED, 8 AI, 13 BIT RESOLUTION, U/I/RESISTANCE/PT100, NI100, NI1000, LG-NI1000, PTC / KTY, 66 MS MODULE UPDATE, 1 X 40 PIN",443,"TEM",1,"Simatic",0.30199999999999999,1]
["6ES73317HF010AB0","SIMATIC S7-300, ANALOG INPUT SM 331, GALVANICALLY ISOLATED, 8 AI, 14 BIT, 0.052 MS/CHANNEL, CURRENT, VOLTAGE, INTERRUPTS, DIAGNOSTICS,1 X 20 PIN, FIT FOR ISOCHRONE MODE IMPROVED DP-CYCLE TIME FOR ISOCHRONE MODE",706,"TEM",1,"Simatic",0.29099999999999998,1]
["6ES73317KB020AB0","SIMATIC S7-300, ANALOG INPUT SM 331, OPTICALLY ISOLATED, 2 AI, 9/12/14 BITS RESOLUTION, U/I/THERMOCOUPLE/RESISTANCE, ALERT, DIAGNOSTICS, 1 X 20 PIN, REMOVE/INSERT W. BACKPLANE BUS",202,"TEM",1,"Simatic",0.246,1]
["6ES73317KF020AB0","SIMATIC S7-300, ANALOG INPUT SM 331, FLOATING, 8AI,  RESOLUTION 9/12/14 BITS, U/I/THERMOCOUPLE/RESISTANCE ALERT, DIAGNOSTICS; 1X20PIN REMOVE/INSERT W. BACKPLANE BUS",646,"TEM",1,"Simatic",0.28899999999999998,1]
["6ES73317NF000AB0","SIMATIC S7-300, ANALOG INPUT SM 331, OPTICALLY ISOLATED, 8 AE; +/-5/10V, 1-5 V, +/-20MA, 0/4 TO 20MA, 16 BIT (55 MS), 1 COMMON POINT(50 V COM.), 1 X 40 PIN",605,"TEM",1,"Simatic",0.312,1]
["6ES73317NF100AB0","SIMATIC S7-300, ANALOG INPUT SM 331, OPTICALLY ISOLATED, 8 AE; +/-5/10V, 1-5 V, +/-20MA, 0/4 TO 20MA, 16 BIT, 1 COMMON POINT(60 V COM.), 4 CHANNEL MODE: 10 MS, 8 CHANNEL MODE: 23-95 MS, 1 X 40 PIN",770,"TEM",1,"Simatic",0.32400000000000001,1]
["6ES73317PE100AB0","SIMATIC S7-300, ANALOG INPUT SM 331, INDIVIDUALLY ISOLATATED AC250V, 6 AI THERMOCOUPLE, TYPE B, E, J, K, L, N, R, S, T VOLTAGE: +/-25MV BIS +/-1V 16 BIT, 50 MS, 1 X 40 PIN",935,"TEM",1,"Simatic",0.33,1]
["6ES73317PF010AB0","SIMATIC S7-300, ANALOG INPUT SM 331, OPT. ISOL.,2/3/4 WIRE, 8AI, RESISTANCE, PT100/200/1000 NI100/120/200/500/1000, CU10, PLUS CHARACTERISTICS ACCORDING TO GOST STANDARD 16 (INTERN 24) BIT, 50MS, 1 X 40 PIN",770,"TEM",1,"Simatic",0.34200000000000003,1]
["6ES73317PF110AB0","SIMATIC S7-300, ANALOG INPUT SM 331, OPTICALLY ISOLATATED, 8 AI THERMOCOUPLE, TYPE B, E, J, K, L, N, R, S, T TXK/TXK(L) ACCORDING GOST 16 BIT, 50 MS, 1 X 40 PIN",770,"TEM",1,"Simatic",0.32900000000000001,1]
["6ES73325HB010AB0","SIMATIC S7-300, ANALOG OUTPUT SM 332, FLOATING, 2 AO, U/I; 11/12 BITS RESOL., 20 PIN., REMOVE/INSERT WITH ACTIVE BACKPLANE BUS",336,"TEM",1,"Simatic",0.252,1]
["6ES73325HD010AB0","SIMATIC S7-300, ANALOG OUTPUT SM 332, OPTICALLY ISOLATED, 4 AO, U/I; DIAGNOSTICS; RESOLUTION 11/12 BITS, 20 PIN, REMOVE/INSERT W. ACTIVE, BACKPLANE BUS",538,"TEM",1,"Simatic",0.252,1]
["6ES73325HF000AB0","SIMATIC S7-300, ANALOG OUTPUT SM 332, OPTICALLY ISOLATED, 8 AO, U/I; DIAGNOSTICS; RESOLUTION 11/12 BITS, 40 PIN, REMOVE/INSERT W. ACTIVE, BACKPLANE BUS",1003,"TEM",1,"Simatic",0.32800000000000001,1]
["6ES73327ND020AB0","SIMATIC S7,SM 332 ANALOG OUTPUT CHANNEL TO CHANNEL ISOLATION, 4 AO, 16 BIT RESOLUTION, 0-10V, 1-5V, +/-10V, +/-20MA, 0/4 - 20MA, 20 PIN, FIT FOR ISOCHRONE MODE IMPROVED DP-CYCLE TIME FOR ISOCHRONE MODE",665,"TEM",1,"Simatic",0.29499999999999998,1]
["6ES73340CE010AA0","SIMATIC S7, ANALOG INPUT/OUTPUT SM 334, NON-ISOLATED, 4 AI/2 AO, 1 X 20 PIN, REMOVE AND INSERT WITH BACKPLAIN BUS",396,"TEM",1,"Simatic",0.24399999999999999,1]
["6ES73340KE000AB0","SIMATIC S7-300, ANALOG MODULE SM 334, OPTICALLY ISOLATED, 4AE/2AA, 12 BIT, 0-10V F. PT100 (CLIMAT RANGE -120 - 155 DEGR.) AND 10 KOHM MEASURING RANGE, 1 X 20 PIN",396,"TEM",1,"Simatic",0.23899999999999999,1]
["6ES73364GE000AB0","SIMATIC S7, ANALOG  INPUT SM336 6 AI; 15 BIT; FAILSAFE ANALOG  INPUTS FOR SIMATIC SAFETY, WITH HART SUPPORT, UP TO CATEGORY 4 (EN954-1)/ SIL3 (IEC61508)/PLE (ISO13849), 1 X 20 PIN,",878,"TEM",1,"Simatic",0.34,1]
["6ES73384BC010AB0","SIMATIC S7-300, SIGNAL. MODULE FOR 3 SSI SENSORS FOR READ-IN OF POSITIONING VALUE WITH 2 FREEZE INPUTS , 1 X 20 PIN, SUPPORTS ISOCHRONE MODE",318,"TEM",1,"Simatic",0.25,1]
["6ES73401AH020AE0","SIMATIC S7-300, CP 340 COMMUNICATION PROCESSOR WITH RS232C INTERFACE (V.24) INCL. CONFIG. PACKAGE ON CD",429,"TEM",1,"Simatic",0.35499999999999998,1]
["6ES73401BH020AE0","SIMATIC S7-300, CP 340 COMMUNICATION PROCESSOR WITH 20MA INTERFACE (TTY) INCL. CONFIG. PACKAGE ON CD",569,"TEM",1,"Simatic",0.35299999999999998,1]
["6ES73401CH020AE0","SIMATIC S7-300, CP 340 COMMUNICATION PROCESSOR WITH RS422/485 INTERFACE INCL. CONFIG. PACKAGE ON CD",569,"TEM",1,"Simatic",0.36,1]
["6ES73411AH020AE0","SIMATIC S7-300, CP341 COMMUNICATION PROCESSOR WITH RS232C INTERFACE (V.24) INCL. CONFIG. PACKAGE ON CD",863,"TEM",1,"Simatic",0.30299999999999999,1]
["6ES73411BH020AE0","SIMATIC S7-300, CP341 COMMUNICATION PROCESSOR WITH 20MA INTERFACE (TTY) INCL. CONFIG. PACKAGE ON CD",927,"TEM",1,"Simatic",0.307,1]
["6ES73411CH020AE0","SIMATIC S7-300, CP341 COMMUNICATION PROCESSOR WITH RS422/485 INTERFACE INCL. CONFIG. PACKAGE ON CD",927,"TEM",1,"Simatic",0.308,1]
["6ES73501AH030AE0","SIMATIC S7-300, COUNTER MODULE FM 350-1 FOR S7-300, COUNTER FUNCTIONS UP TO 500 KHZ 1 CHANNEL FOR CONNECTION OF 5V AND 24V INCREMENTAL ENCODERS ISOCHRON MODE, MEASUREMENT MODE INCL. CONFIG. PACKAGE ON CD",429,"TEM",1,"Simatic",0.28299999999999997,1]
["6ES73502AH010AE0","SIMATIC S7-300, COUNTER MODULE FM 350-2, 8 CHANNELS, 20 KHZ, 24V ENCODER FOR COUNTING, MEASURING FREQUENCIES, SPEED MEASUREMENT, PERIOD DURATION MEASUREMENT AND PROPORTIONING INCL. CONFIG. PACKAGE AND ELECTRONIC DOCU ON CD",987,"TEM",1,"Simatic",0.48299999999999998,1]
["6ES73511AH020AE0","SIMATIC S7-300, FM 351 POSITIONING MODULE FOR RAPID/ CREEP FEED DRIVE INCL. CONFIG. PACKAGE ON CD",769,"TEM",1,"Simatic",0.496,1]
["6ES73521AH020AE0","SIMATIC S7-300, FM 352 ELECTRON. CAM-OPERATED CONTROL INCL. CONFIG. PACKAGE ON CD",810,"TEM",1,"Simatic",0.46800000000000003,1]
["6ES73525AH010AE0","SIMATIC S7-300,  FM352-5 WITH SINK OUT, HIGH SPEED BOOLEAN PROCESSOR, FOR HIGH-SPEED LOGIC OPERATION 12 DI, 8 DO, 1 ENCODER INTERF. FOR RS422 INCR./SSI ENCODER",1036,"TEM",1,"Simatic",0.53700000000000003,1]
["6ES73525AH110AE0","SIMATIC S7-300,  FM352-5 WITH SRC OUT, HIGH SPEED BOOLEAN PROCESSOR, FOR HIGH-SPEED LOGIC OPERATION 12 DI, 8 DO, 1 ENCODER INTERF. FOR RS422 INCR./SSI ENCODER",1132,"TEM",1,"Simatic",0.52600000000000002,1]
["6ES73550VH100AE0","SIMATIC S7-300, CONROL MODULE FM 355 C, 4 CHANNELS, CONTIN. 4 AI + 8 DI + 4 AO INCL. MULTI-LANG CONFIG. PACK., MANUAL AND  GETTING STARTED (GER/EN/FR/IT) ON CD-ROM",1052,"TEM",1,"Simatic",0.57899999999999996,1]
["6ES73551VH100AE0","SIMATIC S7-300, CONTROL MODULE FM 355 S, 4 CHANNELS, STEP AND PULSE, 4 AI + 8 DI + 8 DO INCL. MULTI-LANG CONFIG. PACK., MANUAL AND  GETTING STARTED (GER/EN/FR/IT) ON CD-ROM",911,"TEM",1,"Simatic",0.57299999999999995,1]
["6ES73552CH000AE0","SIMATIC S7-300, TEMPERATURE CONTROL MODULE FM 355-2 C, 4 CHANNELS, CONTIN. 4 AI + 8 DI + 4 AO INCL. MULTI-LANG CONFIG. PACK., MANUAL AND  GETTING STARTED (GER/EN/IT) ON CD-ROM",972,"TEM",1,"Simatic",0.56799999999999995,1]
["6ES73552SH000AE0","SIMATIC S7-300, TEMPERATURE CONTROL MODULE FM 355 S, 4 CHANNELS, STEP AND PULSE, 4 AI + 8 DI + 8 DO INCL. MULTI-LANG CONFIG. PACK., MANUAL AND  GETTING STARTED (GER/EN/IT) ON CD-ROM",840,"TEM",1,"Simatic",0.56999999999999995,1]
["6ES73603AA010AA0","SIMATIC S7-300,INTERFACE MODULE IM 360 IN CENTRAL RACK FOR CONNECTING MAX. 3 EXPANSION RACKS, WITH K-BUS",198,"TEM",1,"Simatic",0.245,1]
["6ES73613CA010AA0","SIMATIC S7-300,INTERFACE MODULE IM 361 IN EXPANSION RACK FOR CONNECTING TO CENTRAL RACK (IM360),24 V DC SUPPLY VOLTAGE, WITH K-BUS",226,"TEM",1,"Simatic",0.40699999999999997,1]
["6ES73650BA010AA0","SIMATIC S7-300,INTERFACE MODULE IM 365 FOR CONNECTING AN EXPANSION RACK, W/O K-BUS, 2 MODULES + CONNECTING CABLE 1M",140,"TEM",1,"Simatic",0.59899999999999998,1]
["6ES73683BB010AA0","SIMATIC S7-300, CONNECTING CABLE BETWEEN IM 360/IM 361 LENGTH: 1M",63,"TEM",1,"Simatic",0.33500000000000002,1]
["6ES73683BC510AA0","SIMATIC S7-300, CONNECTING CABLE BETWEEN IM 360/IM 361 LENGTH: 2.5M",84.4,"TEM",1,"Simatic",0.47799999999999998,1]
["6ES73683BF010AA0","SIMATIC S7-300, CONNECTING CABLE BETWEEN IM 360/IM 361 LENGTH: 5M",113,"TEM",1,"Simatic",0.76,1]
["6ES73683CB010AA0","SIMATIC S7-300, CONNECTING CABLE BETWEEN IM 360/IM 361 LENGTH: 10M",134,"TEM",1,"Simatic",1.323,1]
["6ES73700AA010AA0","SIMATIC S7-300, DUMMY MODULE DM 370, FOR USE WITH MODULE EXCHANGE",93.5,"TEM",1,"Simatic",0.22,1]
["6ES73742XH010AA0","SIMATIC S7-300,SIMULATOR MODULE SM 374, FOR SIMULATING 16 INPUTS OR 16 OUTPUTS RESP. 8 INPUTS AND 8 OUTPUTS; 16 SWITCHES, 16 LED",240,"TEM",1,"Simatic",0.247,1]
["6ES73900AA000AA0","SIMATIC S7-300, BUS CONNECTOR (SPARE PART)",6.9,"TEM",1,"Simatic",1.2999999999999999E-2,1]
["6ES73901AB600AA0","SIMATIC S7-300, RAIL L=160MM",20.3,"TEM",1,"Simatic",0.22700000000000001,0]
["6ES73901AE800AA0","SIMATIC S7-300, RAIL L=480MM",31.5,"TEM",1,"Simatic",0.65400000000000003,0]
["6ES73901AF300AA0","SIMATIC S7-300, RAIL L=530MM",37.800000000000004,"TEM",1,"Simatic",0.73299999999999998,0]
["6ES73901AJ300AA0","SIMATIC S7-300, RAIL L=830MM",50.7,"TEM",1,"Simatic",1.1000000000000001,0]
["6ES73901BC000AA0","SIMATIC S7-300, RAIL L=2000MM",84.4,"TEM",1,"Simatic",2.64,0]
["6ES73905AA000AA0","SIMATIC S7, SHIELD CONNECTING ELEMENT 80MM WIDE, WITH 2 ROWS FOR 4 SHIELDED TERMINALS EACH",13.9,"TEM",1,"Simatic",9.4E-2,0]
["6ES73905AB000AA0","SIMATIC S7, TERMINAL ELEMENT F. 2 CABLES W. 2 - 6MM IN DIA. 2 PIECES PER PACKAGING UNIT",10.4,"ΠΑΚ",1,"Simatic",2.2000000000000002E-2,0]
["6ES73905BA000AA0","SIMATIC S7, TERMINAL ELEMENT F. 1 CABLE W. 3...8MM IN DIA. 2 PIECES PER PACKAGING UNIT",10.4,"ΠΑΚ",1,"Simatic",0.02,0]
["6ES73905CA000AA0","SIMATIC S7, TERMINAL ELEMENT F. 1 CABLE W. 4...13MM IN DIA. 2 PIECES PER PACKAGING UNIT",10.4,"ΠΑΚ",1,"Simatic",3.5000000000000003E-2,0]
["6ES73911AA000AA0","SIMATIC S7-300, SPARE PART PLUG FOR 24V SUPPLY FOR S7-300 CPUS AND FM352-5 10 PIECES PER PACKAGING UNIT",30,"ΠΑΚ",1,"Simatic",6.3E-2,1]
["6ES73921AJ000AA0","SIMATIC S7-300, FRONT CONNECTOR FOR SIGNAL MODULES WITH SCREW CONTACTS, 20-PIN",24.6,"TEM",1,"Simatic",6.9000000000000006E-2,1]
["6ES73921AJ001AB0","SIMATIC S7-300, FRONT CONNECTOR FOR SIGNAL MODULES WITH SCREW CONTACTS, 20-PIN 100 PIECES PER PACKAGING UNIT",2460,"ΠΑΚ",1,"Simatic",6.18,0]
["6ES73921AM000AA0","SIMATIC S7-300,FRONT CONNECTOR WITH SCREW CONTACTS, 40-PIN",38.900000000000006,"TEM",1,"Simatic",0.13400000000000001,1]
["6ES73921AM001AB0","SIMATIC S7-300,FRONT CONNECTOR WITH SCREW CONTACTS, 40-PIN 100 PIECES PER PACKAGING UNIT",3863,"ΠΑΚ",1,"Simatic",12.84,0]
["6ES73921AN000AA0","S7-300, TERMINAL BLOCK WITH SCREW-TYPE TERMINALS FOR 64 CHANNEL MODULES OF S7-300, 2 PIECES PER PACKAGING UNIT",82.300000000000011,"ΠΑΚ",1,"Simatic",0.26600000000000001,1]
["6ES73921BJ000AA0","SIMATIC S7-300, FRONT CONNECTOR FOR SIGNAL MODULES WITH SPRING CONTACTS, 20-PIN",24.6,"TEM",1,"Simatic",0.06,1]
["6ES73921BJ001AB0","SIMATIC S7-300, FRONT CONNECTOR FOR SIGNAL MODULES WITH SPRING CONTACTS, 20-PIN 100 PIECES PER PACKAGING UNIT",2460,"ΠΑΚ",1,"Simatic",5.2,0]
["6ES73921BM010AA0","SIMATIC S7-300, FRONT CONNECTOR FOR SIGNAL MODULES WITH SPRING CONTACTS, 40-PIN,",38.900000000000006,"TEM",1,"Simatic",0.122,1]
["6ES73921BM011AB0","SIMATIC S7-300, FRONT CONNECTOR FOR SIGNAL MODULES WITH SPRING CONTACTS, 40-PIN 100 PIECES PER PACKAGING UNIT",3863,"ΠΑΚ",1,"Simatic",0.08,0]
["6ES73921BN000AA0","S7-300, TERMINAL BLOCK WITH SPRING-LOAD TERMINALS FOR 64 CHANNEL MODULES OF S7-300, 2 PIECES PER PACKAGING UNIT",92.300000000000011,"ΠΑΚ",1,"Simatic",0.26600000000000001,1]
["6ES73922AX000AA0","SIMATIC S7-300, 10 DIN A4 LABELLING SHEETS COLOR: PETROL, 10 LABELLING STRIPS/SHEETS FOR SIGNAL MODULES (16 CHANNELS), MATERIAL: MEMBRANE, PREPERFO- RATED, FOR PRINTING ON A LASER PRINTER, 10 SHEETS PER PACKAGING UNIT",54,"ΠΑΚ",1,"Simatic",0.224,0]
["6ES73922AX100AA0","SIMATIC S7-300, 10 DIN A4 LABELLING SHEETS COLOR: PETROL, 10 LABELLING STRIPS/SHEETS FOR SIGNAL MODULES (32 CHANNELS), MATERIAL: MEMBRANE, PREPERFO- RATED, FOR PRINTING ON A LASER PRINTER, 10 SHEETS PER PACKAGING UNIT",54,"ΠΑΚ",1,"Simatic",0.214,0]
["6ES73922BX000AA0","SIMATIC S7-300, 10 DIN A4 LABELLING SHEETS COLOR: LIGHT-BEIGE, 10 LABELLING STRIPS/SHEETS FOR SIGNAL MODULES (16 CHANNELS), MATERIAL: MEMBRANE, PREPERFO- RATED, FOR PRINTING ON A LASER PRINTER, 10 SHEETS PER PACKAGING UNIT",54,"ΠΑΚ",1,"Simatic",0.22600000000000001,0]
["6ES73922BX100AA0","SIMATIC S7-300, 10 DIN A4 LABELLING SHEETS COLOR: LIGHT-BEIGE, 10 LABELLING STRIPS/SHEETS FOR SIGNAL MODULES (32 CHANNELS), MATERIAL: MEMBRANE, PREPERFO- RATED, FOR PRINTING ON A LASER PRINTER, 10 SHEETS PER PACKAGING UNIT",54,"ΠΑΚ",1,"Simatic",0.223,0]
["6ES73922CX000AA0","SIMATIC S7-300, 10 DIN A4 LABELLING SHEETS COLOR: YELLOW, 10 LABELLING STRIPS/SHEETS FOR SIGNAL MODULES (16 CHANNELS), MATERIAL: MEMBRANE, PREPERFO- RATED, FOR PRINTING ON A LASER PRINTER, 10 SHEETS PER PACKAGING UNIT",54,"ΠΑΚ",1,"Simatic",0.23400000000000001,0]
["6ES73922CX100AA0","SIMATIC S7-300, 10 DIN A4 LABELLING SHEETS COLOR: YELLOW, 10 LABELLING STRIPS/SHEETS FOR SIGNAL MODULES (32 CHANNELS), MATERIAL: MEMBRANE, PREPERFO- RATED, FOR PRINTING ON A LASER PRINTER, 10 SHEETS PER PACKAGING UNIT",54,"ΠΑΚ",1,"Simatic",0.222,0]
["6ES73922DX000AA0","SIMATIC S7-300, 10 DIN A4 LABELLING SHEETS COLOR: RED, 10 LABELLING STRIPS/SHEETS FOR SIGNAL MODULES (16 CHANNELS), MATERIAL: MEMBRANE, PREPERFO- RATED, FOR PRINTING ON A LASER PRINTER, 10 SHEETS PER PACKAGING UNIT",54,"ΠΑΚ",1,"Simatic",0.22500000000000001,0]
["6ES73922DX100AA0","SIMATIC S7-300, 10 DIN A4 LABELLING SHEETS COLOR: RED, 10 LABELLING STRIPS/SHEETS FOR SIGNAL MODULES (32 CHANNELS), MATERIAL: MEMBRANE, PREPERFO- RATED, FOR PRINTING ON A LASER PRINTER, 10 SHEETS PER PACKAGING UNIT",54,"ΠΑΚ",1,"Simatic",0.22800000000000001,0]
["6ES73922XX000AA0","SIMATIC S7-300, LABELING STRIPS (SPARE PART), FOR MODULES WITH FRONT CONNECTOR 20-PIN, 10 PIECES PER PACKAGING UNIT",7,"ΠΑΚ",1,"Simatic",8.9999999999999993E-3,0]
["6ES73922XX100AA0","SIMATIC S7-300, LABELING STRIPS (SPARE PART), FOR MODULES WITH FRONT CONNECTOR 40-PIN, 10 PIECES PER PACKAGING UNIT",7,"ΠΑΚ",1,"Simatic",7.0000000000000001E-3,0]
["6ES73922XX200AA0","SIMATIC S7-300,LABELLING STRIPS FOR F -  MODULES (SPARE PART) 10 PIECES PER PACKAGING UNIT",10.9,"ΠΑΚ",1,"Simatic",7.0000000000000001E-3,0]
["6ES73922XY000AA0","SIMATIC S7-300, LABELING COVER (SPARE PART), FOR MODULES WITH FRONT CONNECTOR 20-PIN, 10 PIECES PER PACKAGING UNIT",7,"ΠΑΚ",1,"Simatic",8.9999999999999993E-3,0]
["6ES73922XY100AA0","SIMATIC S7-300, LABELING COVER (SPARE PART), FOR MODULES WITH FRONT CONNECTOR 40-PIN, 10 PIECES PER PACKAGING UNIT",7,"ΠΑΚ",1,"Simatic",7.0000000000000001E-3,0]
["6ES73922XY200AA0","SIMATIC S7-300, LABELL. COVER FOR F - MODULES (SPARE PART) 10 PIECES PER PACKAGING UNIT",9.2000000000000011,"ΠΑΚ",1,"Simatic",7.0000000000000001E-3,0]
["6ES73924BB000AA0","S7-300 CONNECTING CABLE FOR 64 CHANNEL MODULES, LENGTH: 1M 2 PIECES PER PACKAGING UNIT",63,"ΠΑΚ",1,"Simatic",0.42,1]
["6ES73924BC500AA0","S7-300 CONNECTING CABLE FOR 64 CHANNEL MODULES, LENGTH: 2.5M 2 PIECES PER PACKAGING UNIT",75.400000000000006,"ΠΑΚ",1,"Simatic",0.78,1]
["6ES73924BF000AA0","S7-300 CONNECTING CABLE FOR 64 CHANNEL MODULES, LENGTH: 5M 2 PIECES PER PACKAGING UNIT",126,"ΠΑΚ",1,"Simatic",1.57,1]
["6ES73934AA000AA0","SIMATIC S7-300, CABLE CELL LK 393 FOR EX (I) MODULES L+ AND M INTRINSICALLY SAFE CONNECTIONS TO TERMINALS 5 PIECES PER PACKAGING UNIT",13.9,"ΠΑΚ",1,"Simatic",3.4000000000000002E-2,0]
["6ES73934AA100AA0","SIMATIC S7-300, CABLE CELL LK 393 FOR F - MODULES L+ AND M FAILSAFE CONNECTIONS TO TERMINALS, 5 PIECES PER PACKAGING UNIT",14.200000000000001,"ΠΑΚ",1,"Simatic",5.0000000000000001E-3,1]
["6ES75050KA000AB0","SIMATIC S7-1500, SYSTEM POWER SUPPLY PS 25W 24V DC, SUPPLIES THE OPERATING VOLTAGE FOR THE S7-1500 VIA THE BACKPLANE BUS",195,"TEM",1,"Simatic",0.36499999999999999,1]
["6ES75050RA000AB0","SIMATIC S7-1500, SYSTEM POWER SUPPLY PS 60W 24/48/60V DC, SUPPLIES THE OPERATING VOLTAGE FOR THE S7-1500 VIA THE BACKPLANE BUS",483,"TEM",1,"Simatic",0.66400000000000003,1]
["6ES75070RA000AB0","SIMATIC S7-1500, SYSTEM POWER SUPPLY PS 60W 120/230V AC/DC, SUPPLIES THE OPERATING VOLTAGE FOR THE S7-1500 VIA THE BACKPLANE BUS",483,"TEM",1,"Simatic",0.65500000000000003,1]
["6ES75101DJ010AB0","SIMATIC DP, CPU 1510SP-1 PN FOR ET 200SP, CENTRAL PROCESSING UNIT WITH WORKING MEMORY 100 KB FOR PROGRAM AND 750 KB FOR DATA, 1. INTERFACE: PROFINET IRT WITH 3 PORT SWITCH, 72 NS BIT-PERFORMANCE, SIMATIC MEMORY CARD NECESSARY, BUSADAPTER NECESSARY FOR PORT 1 AND 2",611,"TEM",1,"Simatic",0.40400000000000003,1]
["6ES75101SJ010AB0","SIMATIC DP, CPU 1510SP F-1 PN FOR ET 200SP, CENTRAL PROCESSING UNIT WITH WORKING MEMORY 150 KB FOR PROGRAM AND 750 KB FOR DATA, 1. INTERFACE: PROFINET IRT WITH 3 PORT SWITCH, 72 NS BIT-PERFORMANCE, SIMATIC MEMORY CARD NECESSARY, BUSADAPTER NECESSARY FOR PORT 1 AND 2",732,"TEM",1,"Simatic",0.5,1]
["6ES75111AK010AB0","SIMATIC S7-1500, CPU 1511-1 PN, CENTRAL PROCESSING UNIT WITH WORKING MEMORY 150 KB FOR PROGRAM AND 1 MB FOR DATA, 1. INTERFACE: PROFINET IRT WITH 2 PORT SWITCH, 60 NS BIT-PERFORMANCE, SIMATIC MEMORY CARD NECESSARY",664,"TEM",1,"Simatic",0.50700000000000001,1]
["6ES75111CK000AB0","SIMATIC S7-1500 COMPACT CPU CPU 1511C-1PN, CENTRAL PROCESSING UNIT WITH WORKING MEMORY 175 KB FOR PROGRAM AND 1 MB FOR DATA, 16 DIGITAL INPUTS, 16 DIGITAL OUTPUTS, 5 ANALOG INPUTS, 2 ANALOG OUTPUTS, 6 HIGH SPEED COUNTERS, 4 HIGH SPEED COUNTERS FOR PTO/PWM/FREQUENZY OUTPUT 1. INTERFACE: PROFINET IRT WITH 2 PORT SWITCH, 60 NS BIT-PERFORMANCE, INCL. FRONT CONNECTOR PUSH-IN, SIMATIC MEMORY CARD NECESSARY",1232,"TEM",1,"Simatic",1.2669999999999999,1]
["6ES75111CK004YB5","SIMATIC S7-1500, STARTERKIT, CONSISTING OF: CPU 1511C-1 PN, POWER SUPPLY PM1507, 24V/3A, MOUNTING RAIL 160MM, SIMATIC MEMORY CARD, 4 MB, ETHERNET CABLE. STEP 7 V14 PROFESSIONAL TRIAL365-LICENSE, INFO MATERIAL, IN SYSTAINER",2121,"TEM",1,"Simatic",3.6,0]
["6ES75111FK010AB0","SIMATIC S7-1500F, CPU 1511F-1 PN, CENTRAL PROCESSING UNIT WITH WORKING MEMORY 225 KB FOR PROGRAM AND 1 MB FOR DATA, 1. INTERFACE: PROFINET IRT WITH 2 PORT SWITCH, 60 NS BIT-PERFORMANCE, SIMATIC MEMORY CARD NECESSARY",907,"TEM",1,"Simatic",0.51300000000000001,1]
["6ES75121CK000AB0","SIMATIC S7-1500 COMPACT CPU CPU 1512C-1 PN, CENTRAL PROCESSING UNIT WITH WORKING MEMORY 250 KB FOR PROGRAM AND 1 MB FOR DATA, 32 DIGITAL INPUTS, 32 DIGITAL OUTPUTS, 5 ANALOG INPUTS, 2 ANALOG OUTPUTS, 6 HIGH SPEED COUNTERS, 4 HIGH SPEED COUNTERS FOR PTO/PWM/FREQUENZY OUTPUT 1. INTERFACE: PROFINET IRT WITH 2 PORT SWITCH, 48 NS BIT-PERFORMANCE, INCL. FRONT CONNECTOR PUSH-IN, SIMATIC MEMORY CARD NECESSARY",1768,"TEM",1,"Simatic",1.5840000000000001,1]
["6ES75121CK004AB1","TRAINING BUNDLE COMPACT CPU 1512C-1 PN CONSISTING OF: S7-1500 CPU 1512C-1 PN, 250 KB / 1 MB, 32 DI, 32 DQ, 5 AI, 2 AQ, SIMATIC MEMORY CARD 24 MB, INCLUSIVE FRONTCONNECTOR, ETHERNET CORD RJ45/RJ45 6M, MOUNTING RAIL, 482 MM, PM 24V/8A, SOFTWARE F. TRAINING STEP 7 V13 ******************************* FOR EDUCATIONAL PURPOSES ONLY",1612,"TEM",1,"Simatic",4.5999999999999996,0]
["6ES75121CK004AB2","TRAINING BUNDLE COMPACT CPU 1512C-1 PN CONSISTING OF: S7-1500 CPU 1512C-1 PN, 250 KB / 1 MB, 32 DI, 32 DQ, 5 AI, 2 AQ, SIMATIC MEMORY CARD 24 MB, INCLUSIVE FRONTCONNECTOR, ETHERNET CORD RJ45/RJ45 6M, MOUNTING RAIL, 482 MM, CP 1542-5 DP, PM 24V/8A, SOFTWARE F. TRAINING STEP 7 V13 ******************************* FOR EDUCATIONAL PURPOSES ONLY",2183,"TEM",1,"Simatic",4.9000000000000004,0]
["6ES75121CK004AB6","TRAINING BUNDLE COMPACT CPU 1512C-1 PN CONSISTING OF: S7-1500 CPU 1512C-1 PN, 250 KB / 1 MB, 32 DI, 32 DQ, 5 AI, 2 AQ, SIMATIC MEMORY CARD 24 MB, INCLUSIVE FRONTCONNECTOR, ETHERNET CORD RJ45/RJ45 6M, MOUNTING RAIL, 482 MM, SOFTWARE F. TRAINING STEP 7 V13 ******************************* FOR EDUCATIONAL PURPOSES ONLY",1449,"TEM",1,"Simatic",3.8,0]
["6ES75121CK004AB7","TRAINING BUNDLE COMPACT CPU 1512C-1 PN CONSISTING OF: S7-1500 CPU 1512C-1 PN, 250 KB / 1 MB, 32 DI, 32 DQ, 5 AI, 2 AQ, SIMATIC MEMORY CARD 24 MB, INCLUSIVE FRONTCONNECTOR, ETHERNET CORD RJ45/RJ45 6M, MOUNTING RAIL, 482 MM, CP 1542-5 DP, SOFTWARE F. TRAINING STEP 7 V13 ******************************* FOR EDUCATIONAL PURPOSES ONLY",2020,"TEM",1,"Simatic",4.0999999999999996,0]
["6ES75121DK010AB0","SIMATIC DP, CPU 1512SP-1 PN FOR ET 200SP, CENTRAL PROCESSING UNIT WITH WORKING MEMORY 200 KB FOR PROGRAM AND 1 MB FOR DATA, 1. INTERFACE: PROFINET IRT WITH 3 PORT SWITCH, 48 NS BIT-PERFORMANCE, SIMATIC MEMORY CARD NECESSARY, BUSADAPTER NECESSARY FOR PORT 1 AND 2",783,"TEM",1,"Simatic",0.5,1]
["6ES75121SK004AB2","TRAINING BUNDLE CPU 1512SP F-1 PN CONSISTING OF: S7-1500 CPU 1512SP F-1 PN, 300 KB / 1 MB, 1X BUS ADAPTER BA 2XRJ45, 16 DI, 16 DQ, 4X BASE UNITS, ETHERNET CORD RJ45/RJ45 6M, MOUNTING RAIL, 483 MM, LABELING STRIPS, COLOUR CODED LABELS SOFTWARE F. TRAINING STEP 7 V13 ******************************* FOR EDUCATIONAL PURPOSES ONLY",1106,"TEM",1,"Simatic",2.6,0]
["6ES75121SK010AB0","SIMATIC DP, CPU 1512SP F-1 PN FOR ET 200SP, CENTRAL PROCESSING UNIT WITH WORKING MEMORY 300 KB FOR PROGRAM AND 1 MB FOR DATA, 1. INTERFACE: PROFINET IRT WITH 3 PORT SWITCH, 48 NS BIT-PERFORMANCE, SIMATIC MEMORY CARD NECESSARY, BUSADAPTER NECESSARY FOR PORT 1 AND 2",1016,"TEM",1,"Simatic",0.41499999999999998,1]
["6ES75131AL004AB0","TRAINING BUNDLE CPU 1513-1 PN CONSISTING OF: S7-1500 CPU 1513-1 PN , 300 KB / 1,5 MB, 32 DI, 32 DQ SIMATIC MEMORY CARD 24 MB, 2 X 40 POL FRONTCONNECTOR ETHERNET CORD RJ45/RJ45 6M, MOUNTING RAIL, 482 MM PM 24V/8A ******************************* FOR EDUCATIONAL PURPOSES ONLY OFFER LIMITED UNTIL 12-31-2015",1628,"TEM",1,"Simatic",3,0]
["6ES75131AL004AB5","TRAINING BUNDLE CPU 1513-1 PN (OEM) CONSISTING OF: S7-1500 CPU 1513-1 PN , 300 KB / 1,5 MB, 32 DI, 32 DQ SIMATIC MEMORY CARD 24 MB, 2 X 40 POL FRONTCONNECTOR ETHERNET CORD RJ45/RJ45 6M, MOUNTING RAIL, 482 MM ******************************* FOR EDUCATIONAL PURPOSES ONLY OFFER LIMITED UNTIL 12-31-2015",1465,"TEM",1,"Simatic",2.1,0]
["6ES75131AL010AB0","SIMATIC S7-1500, CPU 1513-1 PN, CENTRAL PROCESSING UNIT WITH WORKING MEMORY 300 KB FOR PROGRAM AND 1.5 MB FOR DATA, 1. INTERFACE: PROFINET IRT WITH 2 PORT SWITCH, 40 NS BIT-PERFORMANCE, SIMATIC MEMORY CARD NECESSARY",1479,"TEM",1,"Simatic",0.504,1]
["6ES75131FL010AB0","SIMATIC S7-1500F, CPU 1513F-1 PN, CENTRAL PROCESSING UNIT WITH WORKING MEMORY 450 KB FOR PROGRAM AND 1.5 MB FOR DATA, 1. INTERFACE: PROFINET IRT WITH 2 PORT SWITCH, 40 NS BIT-PERFORMANCE, SIMATIC MEMORY CARD NECESSARY",1792,"TEM",1,"Simatic",0.51100000000000001,1]
["6ES75152AM010AB0","SIMATIC S7-1500, CPU 1515-2 PN, CENTRAL PROCESSING UNIT WITH WORKING MEMORY 500 KB FOR PROGRAM AND 3 MB FOR DATA, 1. INTERFACE: PROFINET IRT WITH 2 PORT SWITCH, 2. INTERFACE: PROFINET RT, 30 NS BIT-PERFORMANCE, SIMATIC MEMORY CARD NECESSARY",2207,"TEM",1,"Simatic",0.91500000000000004,1]
["6ES75152FM010AB0","SIMATIC S7-1500F, CPU 1515F-2 PN, CENTRAL PROCESSING UNIT WITH WORKING MEMORY 750 KB FOR PROGRAM AND 3 MB FOR DATA, 1. INTERFACE: PROFINET IRT WITH 2 PORT SWITCH, 2. INTERFACE: PROFINET RT, 30 NS BIT-PERFORMANCE, SIMATIC MEMORY CARD NECESSARY",2589,"TEM",1,"Simatic",0.91600000000000004,1]
["6ES75162GN000AB0","SIMATIC DP, CPU 1516PRO F-2 PN for ET 200pro, Central processing unit with work memory 1.5 MB for program and 5 MB for data, 1. interface: PROFINET IRT with 3-port switch, 2. interface: PROFINET RT, 10 ns bit performance, degree of protection IP65/67 SIMATIC memory card neccessary connection module necessary",3633,"TEM",1,"Simatic",0.7,1]
["6ES75162PN000AB0","SIMATIC DP, CPU 1516PRO-2 PN for ET 200pro, Central processing unit with work memory 1 MB for program and 5 MB for data, 1. interface: PROFINET IRT with 3-port switch, 2. interface: PROFINET RT, 10 ns bit performance, degree of protection IP65/67 SIMATIC memory card neccessary connection module necessary",3255,"TEM",1,"Simatic",0.7,1]
["6ES75163AN004AB3","TRAINING BUNDLE CPU 1516-3 PN/DP CONSISTING OF: S7-1500 CPU 1516-3 PN/DP , 1 MB / 5 MB, 32 DI, 32 DQ, 8 AI, 4 AQ,32 DI, SIMATIC MEMORY CARD 24 MB, 4 X 40 POL FRONTCONNECTOR ETHERNET CORD RJ45/RJ45 6M MOUNTING RAIL, 482 MM PM 24V/8A SOFTWARE F. TRAINING STEP 7 V13 ******************************* FOR EDUCATIONAL PURPOSES ONLY",2015,"TEM",1,"Simatic",4.8,0]
["6ES75163AN004AB8","TRAINING BUNDLE CPU 1516-3 PN/DP (OEM) CONSISTING OF: S7-1500 CPU 1516-3 PN/DP , 1 MB / 5 MB, 32 DI, 32 DQ, 8 AI, 4 AQ,32 DI, SIMATIC MEMORY CARD 24 MB, 2 X 40 POL FRONTCONNECTOR 2 X IDC-CONNECTION 4 X 16-PIN, ETHERNET CORD RJ45/RJ45 6M MOUNTING RAIL, 482 MM SOFTWARE F. TRAINING STEP 7 V13 ******************************* FOR EDUCATIONAL PURPOSES ONLY",1852,"TEM",1,"Simatic",4.8,0]
["6ES75163AN010AB0","SIMATIC S7-1500, CPU 1516-3 PN/DP, CENTRAL PROCESSING UNIT WITH WORKING MEMORY 1 MB FOR PROGRAM AND 5 MB FOR DATA, 1. INTERFACE: PROFINET IRT WITH 2 PORT SWITCH, 2. INTERFACE: PROFINET RT, 3. INTERFACE: PROFIBUS, 10 NS BIT-PERFORMANCE, SIMATIC MEMORY CARD NECESSARY",3570,"TEM",1,"Simatic",0.94,1]
["6ES75163FN004AB2","Training bundle CPU 1516F-3 PN/DP consiSTing of: S7-1500 CPU 1516F-3 PN/DP , 1,5 MB / 5 MB, 32 DI, 32 DQ, 8 AI, 4 AQ, SIMATIC memory card 24 MB, 4 X 40 pin frontconnector Ethernet cord RJ45/RJ45 6m mounting rail, 482 mm PM 24V/8A Software f. Training STEP 7 V13 ******************************* for educational Purposes only",2445,"TEM",1,"Simatic",7,0]
["6ES75163FN004AB8","Training bundle CPU 1516F-3 PN/DP (OEM) consiSTing of: S7-1500 CPU 1516F-3 PN/DP , 1,5 MB / 5 MB, 32 DI, 32 DQ, 8 AI, 4 AQ, SIMATIC memory card 24 MB, 2 x frontconnector 40 pin, 2 X IDC connection 4 x 16-pin, Ethernet cord RJ45/RJ45 6m, mounting rail, 482 mm Software f. Training STEP 7 V13 ******************************* for educational purposes only",2281,"TEM",1,"Simatic",5.2,0]
["6ES75163FN010AB0","SIMATIC S7-1500F, CPU 1516F-3 PN/DP, CENTRAL PROCESSING UNIT WITH WORKING MEMORY 1,5 MB FOR PROGRAM AND 5 MB FOR DATA, 1. INTERFACE: PROFINET IRT WITH 2 PORT SWITCH, 2. INTERFACE: PROFINET RT, 3. INTERFACE: PROFIBUS, 10 NS BIT-PERFORMANCE, SIMATIC MEMORY CARD NECESSARY",4027,"TEM",1,"Simatic",0.93600000000000005,1]
["6ES75173AP000AB0","SIMATIC S7-1500, CPU 1517-3 PN/DP, CENTRAL PROCESSING UNIT WITH WORKING MEMORY 2 MB FOR PROGRAM AND 8 MB FOR DATA, 1. INTERFACE: PROFINET IRT WITH 2 PORT SWITCH, 2. INTERFACE: PROFINET RT, 3. INTERFACE: PROFIBUS, 2 NS BIT-PERFORMANCE, SIMATIC MEMORY CARD NECESSARY",4620,"TEM",1,"Simatic",2.1389999999999998,1]
["6ES75173FP000AB0","SIMATIC S7-1500F, CPU 1517F-3 PN/DP, CENTRAL PROCESSING UNIT WITH WORKING MEMORY 3 MB FOR PROGRAM AND 8 MB FOR DATA, 1. INTERFACE: PROFINET IRT WITH 2 PORT SWITCH, 2. INTERFACE: PROFINET RT, 3. INTERFACE: PROFIBUS, 2 NS BIT-PERFORMANCE, SIMATIC MEMORY CARD NECESSARY",5205,"TEM",1,"Simatic",2.141,1]
["6ES75184AP000AB0","SIMATIC S7-1500, CPU 1518-4 PN/DP, CENTRAL PROCESSING UNIT WITH WORKING MEMORY 4 MB FOR PROGRAM AND 20 MB FOR DATA, 1. INTERFACE: PROFINET IRT WITH 2 PORT SWITCH, 2. INTERFACE: PROFINET RT, 3. INTERFACE: ETHERNET, 4. INTERFACE: PROFIBUS, 1 NS BIT-PERFORMANCE, SIMATIC MEMORY CARD NECESSARY",6720,"TEM",1,"Simatic",2.1349999999999998,1]
["6ES75184AP003AB0","SIMATIC S7-1500, CPU 1518-4 PN/DP, CENTRAL PROCESSING UNIT WITH ODK RUNTIME INTERFACE, WORKING MEMORY 4 MB FOR PROGRAM AND 20 MB FOR DATA, 1. INTERFACE: PROFINET IRT WITH 2 PORT SWITCH, 2. INTERFACE: PROFINET RT, 3. INTERFACE: ETHERNET, 4. INTERFACE: PROFIBUS, 1 NS BIT-PERFORMANCE, SIMATIC MEMORY CARD NECESSARY",7560,"TEM",1,"Simatic",2.1349999999999998,1]
["6ES75184FP000AB0","SIMATIC S7-1500F, CPU 1518F-4 PN/DP, CENTRAL PROCESSING UNIT WITH WORKING MEMORY 6 MB FOR PROGRAM AND 20 MB FOR DATA, 1. INTERFACE: PROFINET IRT WITH 2 PORT SWITCH, 2. INTERFACE: PROFINET RT, 3. INTERFACE: ETHERNET, 4. INTERFACE: PROFIBUS, 1 NS BIT-PERFORMANCE, SIMATIC MEMORY CARD NECESSARY",7562,"TEM",1,"Simatic",2.1440000000000001,1]
["6ES75184FP003AB0","SIMATIC S7-1500F, CPU 1518F-4 PN/DP ODK, CENTRAL PROCESSING UNIT WITH SIMATIC S7-1500F, WORKING MEMORY 6 MB FOR PROGRAM AND 20 MB FOR DATA, 1. INTERFACE: PROFINET IRT WITH 2 PORT SWITCH, 2. INTERFACE: PROFINET RT, 3. INTERFACE: ETHERNET, 4. INTERFACE: PROFIBUS, 1 NS BIT-PERFORMANCE, SIMATIC MEMORY CARD NECESSARY",8348,"TEM",1,"Simatic",2.1349999999999998,1]
["6ES75211BH000AB0","SIMATIC S7-1500, DIGITAL INPUT MODULE DI 16xDC 24V HF, 16 CHANNELS IN GROUPS OF 16; INPUT DELAY 0.05 ... 20MS; INPUT TYPE 3 (IEC 61131); DIAGNOSIS, PROCESSALARMS",192,"TEM",1,"Simatic",0.28999999999999998,1]
["6ES75211BH100AA0","SIMATIC S7-1500, DIGITAL INPUT MODULE, DI 16xDC 24V BA, 16 CHANNELS IN GROUPS OF 16; INPUT DELAY TYP. 3.2MS; INPUT TYPE 3 (IEC 61131) INCL. FRONT CONNECTOR PUSH-IN",200,"TEM",1,"Simatic",0.311,1]
["6ES75211BH500AA0","SIMATIC S7-1500, DIGITAL INPUT MODULE DI16 X DC24V BA, SOURCE; 16 CHANNELS IN GROUPS OF 16; INPUT DELAY 3.2MS; INPUT TYPE 3 (IEC 61131)",154,"TEM",1,"Simatic",0.28599999999999998,1]
["6ES75211BL000AB0","SIMATIC S7-1500, DIGITAL INPUT MODULE DI 32xDC 24V HF, 32 CHANNELS IN GROUPS OF 16; INPUT DELAY 0.05... 20MS; INPUT TYPE 3 (IEC 61131); DIAGNOSIS, PROCESSALARMS",301,"TEM",1,"Simatic",0.312,1]
["6ES75211BL100AA0","SIMATIC S7-1500, DIGITAL INPUT MODULE, DI 32xDC 24V BA, 32 CHANNELS IN GROUPS OF 16; INPUT DELAY TYP. 3.2MS; INPUT TYPE 3 (IEC 61131) INCL. FRONT CONNECTOR PUSH-IN",304,"TEM",1,"Simatic",0.35499999999999998,1]
["6ES75211FH000AA0","SIMATIC S7-1500, DIGITAL INPUT MODULE DI 16xAC 230V BA, 16 CHANNELS IN GROUPS OF 4; INPUT DELAY 20MS; INPUT TYPE 1 (IEC 61131)",215,"TEM",1,"Simatic",0.35099999999999998,1]
["6ES75217EH000AB0","SIMATIC S7-1500, DIGITAL INPUT MODULE DI 16 X 24...125V UC HF, 16 CHANNELS IN GROUPS OF 1; INPUT DELAY 0.05 ... 20MS; INPUT TYPE 3 (IEC 61131); DIAGNOSIS, PROCESSALARMS",481,"TEM",1,"Simatic",0.27100000000000002,1]
["6ES75221BF000AB0","SIMATIC S7-1500, DIGITAL OUTPUT MODULE DQ 8xDC 24V/2A HF; 8 CHANNELS IN GROUPS OF 8, 8 A PER GROUP; DIAGNOSIS; SUBSTITUTE VALUE",173,"TEM",1,"Simatic",0.29499999999999998,1]
["6ES75221BH010AB0","SIMATIC S7-1500, DIGITAL OUTPUT MODULE DQ 16 X 24V DC/0.5A HF; 16 CHANNELS IN GROUPS OF 8, 4 A PER GROUP; SINGLE-CHANNEL DIAGNOSIS; SUBSTITUTE VALUE",204,"TEM",1,"Simatic",0.29099999999999998,1]
["6ES75221BH100AA0","SIMATIC S7-1500, DIGITAL OUTPUT MODULE, DQ 16 X 24VDC/0.5A BA; 16 CHANNELS IN GROUPS OF 8, 4 A PER GROUP; INCL. FRONT CONNECTOR PUSH-IN",185,"TEM",1,"Simatic",0.316,1]
["6ES75221BL010AB0","SIMATIC S7-1500, DIGITAL OUTPUT MODULE DQ 32 X 24V DC/0.5A HF; 32 CHANNELS IN GROUPS OF 8, 4 A PER GROUP; SINGLE-CHANNEL DIAGNOSIS; SUBSTITUTE VALUE",428,"TEM",1,"Simatic",0.33900000000000002,1]
["6ES75221BL100AA0","SIMATIC S7-1500, DIGITAL OUTPUT MODULE, DQ 32 X 24VDC/0.5A BA; 32 CHANNELS IN GROUPS OF 8, 4 A PER GROUP; INCL. FRONT CONNECTOR PUSH-IN",370,"TEM",1,"Simatic",0.36699999999999999,1]
["6ES75225EH000AB0","SIMATIC S7-1500, DIGITAL OUTPUT MODULE DQ16x24..48VUC/125V DC/0.5A ST; 16 CHANNELS IN GROUPS OF 1, 0.5A PER GROUP; SUBSTITUTE VALUE; PLEASE NOTE DERATING",717,"TEM",1,"Simatic",0.2,1]
["6ES75225FF000AB0","SIMATIC S7-1500, DIGITAL OUTPUT MODULE DQ 8 X 230VAC,2A ST,TRIAC; 8 CHANNELS IN GROUPS OF 1, 2A PER GROUP; SUBSTITUTE VALUE",214,"TEM",1,"Simatic",0.34599999999999997,1]
["6ES75225FH000AB0","SIMATIC S7-1500, DIGITAL OUTPUT MODULE DQ 16 X 230VAC / 1A ST,TRIAC; 16 CHANNELS IN GROUPS OF 2, 2A PER GROUP; SUBSTITUTE VALUE",353,"TEM",1,"Simatic",0.2,1]
["6ES75225HF000AB0","SIMATIC S7-1500, DIGITAL OUTPUT MODULE DQ 8 X 230VAC/5A ST,RELAY; 8 CHANNELS IN GROUPS OF 1, 5A PER GROUP; DIAGNOSIS; SUBSTITUTE VALUE",320,"TEM",1,"Simatic",0.40500000000000003,1]
["6ES75225HH000AB0","SIMATIC S7-1500, DIGITAL OUTPUT MODULE DQ 16 X 230VAC / 2A ST; RELAY; 16 CHANNELS IN GROUPS OF 2, 4A PER GROUP; DIAGNOSIS; SUBSTITUTE VALUE",342,"TEM",1,"Simatic",0.2,1]
["6ES75231BL000AA0","SIMATIC S7-1500 DIGITAL IN-/OUTPUT MODULE, DI16x 24VDC BA, 16 CHANNELS IN GROUPS OF 16, INPUT DELAY TYP. 3.2MS; INPUT TYPE 3 (IEC 61131), DQ 16X24VDC/0.5A BA; 16 CHANNELS IN GROUPS OF 8; 4A PER GROUP INCL. FRONT CONNECTOR PUSH-IN",388,"TEM",1,"Simatic",0.36,1]
["6ES75261BH000AB0","SIMATIC S7-1500, FAILSAFE DIGITAL INPUT MODULE, F-DI 16X24VDC PROFISAFE; 35 MM WIDTH; UP TO PL E (ISO 13849-1)/ SIL3 (IEC 61508)",630,"TEM",1,"Simatic",0.09,1]
["6ES75262BF000AB0","SIMATIC S7-1500, FAILSAFE DIGITAL OUTPUT MODULE F-DQ 8X24VDC 2A PPM PROFISAFE; 35 MM WIDTH; UP TO PL E (ISO 13849-1)/ SIL3 (IEC 61508)",725,"TEM",1,"Simatic",0.09,1]
["6ES75280AA000AA0","SIMATIC S7-1500, SPARE PART FRONT DOOR FOR 25MM WIDE IO MODUELS, CONSISTING OF: * FRONT DOOR (UNLABELED), * LABEL (FRONT), * WIRING DIAGRAM, 5 PIECES PER PACKAGING UNIT",59,"ΠΑΚ",1,"Simatic",0.21199999999999999,0]
["6ES75280AA007AA0","SIMATIC S7-1500, SPARE PART FRONT DOOR FOR 35MM WIDE IO MODUELS, CONSISTING OF: * FRONT DOOR (UNLABELED), * LABEL (FRONT), * WIRING DIAGRAM, 5 PIECES PER PACKAGING UNIT",59,"ΠΑΚ",1,"Simatic",0.27900000000000003,0]
["6ES75280AA107AA0","SIMATIC S7-1500, SPARE PART FRONT DOOR FOR F-IO MODUELS, CONSISTING OF: * FRONT DOOR (UNLABELED), * LABEL (FRONT, YELLOW FOR F MODULES * WIRING DIAGRAM, 5 PIECES PER PACKAGING UNIT",57.800000000000004,"ΠΑΚ",1,"Simatic",0.27900000000000003,0]
["6ES75280AA607AA0","SIMATIC S7-1500, SPARE PART FRONT DOOR FOR 70MM WIDE POWER SUPPLY 5 PIECES PER PACKAGING UNIT",59,"TEM",1,"Simatic",0.27900000000000003,0]
["6ES75280AA707AA0","SIMATIC ET 200MP, SPARE PART FRONT DOOR FOR IM155-5 (6ES7 155-5AA00-0AB0) 5 PIECES PER PACKAGING UNIT",37.5,"ΠΑΚ",1,"Simatic",0.17599999999999999,0]
["6ES75280AA807AA0","SIMATIC S7-1500, SPARE PART FRONT DOOR FOR 35MM WIDE POWER SUPPLY AND PTP CP 5 PIECES PER PACKAGING UNIT",59,"TEM",1,"Simatic",0.27900000000000003,0]
["6ES75317KF000AB0","SIMATIC S7-1500, ANALOG INPUT MODULE AI 8 X U/I/RTD/TC ST, 16 BITS OF RESOLUTION, ACCURACY 0.3 %; 8 CHANNELS IN GROUPS OF 8; 4 CHANNNELS FOR RTD MEASURING, COMMON MODE VOLTAGE APPR. 10 V; DIAGNOSIS, PROCESSALARMS INCL. INFEED ELEMENT, SHIELD CLAMP AND SHIELD TERMINAL",579,"TEM",1,"Simatic",0.437,1]
["6ES75317NF000AB0","SIMATIC S7-1500, ANALOG INPUT MODULE AI 8 X U/I HF, 16 BITS OF RESOLUTION, ACCURACY 0.1%, 8 CHANNELS IN GROUPS OF 1; COMMON MODE VOLTAGE: 30V AC/60V DC, DIAGNOSIS, PROCESSALARMS; INCL. INFEED ELEMENT, SHIELD CLAMP AND SHIELD TERMINAL",783,"TEM",1,"Simatic",0.3,1]
["6ES75317NF100AB0","SIMATIC S7-1500, ANALOG INPUT MODULE AI 8 X U/I HS, 16 BITS OF RESOLUTION, ACCURACY 0.3 %; 8 CHANNELS IN GROUPS OF 8; COMMON MODE VOLTAGE APPR. 10V; DIAGNOSIS, PROCESSALARMS; 8 CHANNELS IN 0.0625 MS INCL. INFEED ELEMENT, SHIELD CLAMP AND SHIELD TERMINAL",705,"TEM",1,"Simatic",0.42899999999999999,1]
["6ES75317PF000AB0","SIMATIC S7-1500, ANALOG INPUT MODULE AI 8 X U/R/RTD/TC HF, 16 BITS OF RESOLUTION, ACCURACY 0.1%, 8 CHANNELS IN GROUPS OF 1; COMMON MODE VOLTAGE: 30V AC/60V DC, DIAGNOSIS, PROCESSALARMS; INCL. INFEED ELEMENT, SHIELD CLAMP AND SHIELD TERMINAL",885,"TEM",1,"Simatic",0.3,1]
["6ES75317QD000AB0","SIMATIC S7-1500, ANALOG INPUT MODULE AI 4 X U/I/RTD/TC ST, 16 BITS OF RESOLUTION, ACCURACY 0.3 %; 4 CHANNELS IN GROUPS OF 4; 2 CHANNNELS FOR RTD MEASURING, COMMON MODE VOLTAGE APPR. 10 V; DIAGNOSIS, PROCESSALARMS INCL. FRONT CONNECTOR PUSH-IN, FEEDING ELEMENT, SHIELDING ELEMENT, SHIELDING CLAMP",302,"TEM",1,"Simatic",0.38,1]
["6ES75325HD000AB0","SIMATIC S7-1500, ANALOG OUTPUT MODULE AQ 4 X U/I ST; 16 BITS OF RESOLUTION, ACCURACY 0.3 %; 4 CHANNELS IN GROUPS OF 4; DIAGNOSIS, SUBSTITUTE VALUE INCL. INFEED ELEMENT, SHIELD CLAMP AND SHIELD TERMINAL",492,"TEM",1,"Simatic",0.41499999999999998,1]
["6ES75325HF000AB0","SIMATIC S7-1500, ANALOG OUTPUT MODULE AQ 8 X U/I HS 16 BITS OF RESOLUTION, ACCURACY 0.3 %, 8CHANNELS IN GROUPS OF 8, DIAGNOSIS, SUBSTITUTE VALUE 8 CHANNELS IN 0.125 MS INCL. INFEED ELEMENT, SHIELD CLAMP AND SHIELD TERMINAL",705,"TEM",1,"Simatic",0.435,1]
["6ES75325NB000AB0","SIMATIC S7-1500, ANALOG OUTPUT MODULE AQ 2 X U/I ST, 16 BITS OF RESOLUTION, ACCURACY 0.3 %. 2 CHANNELS IN GROUPS OF 2, DIAGNOSIS, SUBSTITUTE VALUE INCL. FRONT CONNECTOR PUSH-IN, FEEDING ELEM., SHIELDING ELEM., SHIELDING CLAMP",259,"TEM",1,"Simatic",0.371,1]
["6ES75325ND000AB0","SIMATIC S7-1500, ANALOG OUTPUT MODULE AQ 4 X U/I HF, 16 BITS OF RESOLUTION, ACCURACY 0.1%, 4 CHANNELS IN GROUPS OF 1; COMMON MODE VOLTAGE: 30V AC/60V DC, DIAGNOSIS, SUBSTITUTE VALUE INCL. INFEED ELEMENT, SHIELD CLAMP AND SHIELD TERMINAL",676,"TEM",1,"Simatic",0.3,1]
["6ES75347QE000AB0","SIMATIC S7-1500, ANALOG IN-/OUTPUT MODULE AI 4X U/I/R/RTD/TC ST; 4 CHANNELS IN GROUPS OF 4 PROCESSALARMS; DIAGNOSTICS AQ 2X U/I ST; 2 CHANNELS IN GROUPS OF 2; SUBSTITUTE VALUE; DIAGNOSTICS; COMMON-MODE-VOLTAGE APPR. 10V; 16BIT; ACCURACY 0.3% INCL. FRONT CONNECTOR PUSH IN, FEEDING ELEMENT, SHIELDING ELE- MENT, SHIELDING CLAMP",560,"TEM",1,"Simatic",0.41799999999999998,1]
["6ES75401AB000AA0","SIMATIC S7-1500, CM PTP RS422/485 BA COMMUNICATION MODULE FOR SERIAL CONNECTION RS422, RS485 FREEPORT, 3964(R), USS, 19200 KBIT/S, 15-PIN SUB-D FEMALE CONNECTOR",531,"TEM",1,"Simatic",0.27300000000000002,1]
["6ES75401AD000AA0","SIMATIC S7-1500, CM PTP RS232 BA COMMUNICATION MODUL FOR SERIAL CONNECTION RS232, FREEPORT, 3964(R), USS, 19200 KBIT/S, 9-PIN SUB-D CONNECTOR",399,"TEM",1,"Simatic",0.26800000000000002,1]
["6ES75411AB000AB0","SIMATIC S7-1500, CM PTP RS422/485 HF COMMUNICATION MODUL FOR SERIAL CONNECTION RS422, RS485, FREEPORT, 3964(R), USS, MODBUS RTU MASTER, SLAVE, 115200 KBIT/S, 15-PIN SUB-D FEMALE CONNECTOR",865,"TEM",1,"Simatic",0.27300000000000002,1]
["6ES75411AD000AB0","SIMATIC S7-1500, CM PTP RS232 HF COMMUNICATION MODUL FOR SERIAL CONNECTION RS232, FREEPORT, 3964(R), USS, MODBUS RTU MASTER, SLAVE, 115200 KBIT/S, 9-PIN SUB-D CONNECTOR",805,"TEM",1,"Simatic",0.26900000000000002,1]
["6ES75455DA000AB0","SIMATIC DP, CM PROFIBUS DP FOR ET 200SP CPU MODULE WITH PROFIBUS DP INTERF. (9 PIN SUB-D, FEMALE) DP-MASTER FOR 125 DP-SLAVES",415,"TEM",1,"Simatic",0.104,1]
["6ES75501AA000AB0","SIMATIC S7-1500, TM COUNT 2X24V COUNTING MODULE, 2 CHANNELS FOR 24V INCREMENTAL ENCODER OR 24V PULSES, 3DI, 2DQ PER CHANNEL",482,"TEM",1,"Simatic",0.39500000000000002,1]
["6ES75511AB000AB0","SIMATIC S7-1500, TM POSINPUT 2 COUNTING AND POSITON DETECTION MODULE, FOR RS422 INCREMENTAL ENCODER OR SSI ABSOLUTE ENCODER, 2 CHANNELS, 2DI,2DQ PER CHANNEL",482,"TEM",1,"Simatic",0.45300000000000001,1]
["6ES75521AA000AB0","SIMATIC S7-1500, TM TIMER DIDQ 16X24V TIME BASED DIGITAL INPUTS AND OUTPUTS MAX. 8DI, 16DQ MAX. 16 WITH TIMESTAMP COUNT, PWM, OVERSAMPLING",482,"TEM",1,"Simatic",0.42399999999999999,1]
["6ES75900AA000AA0","SIMATIC S7-1500, SPARE PART, U-TYPE-CONNECTOR FOR CONNECTING IO MODULES (SELF CONFIGURING BACKPLANE) 5 PIECES PER PACKAGING UNIT",52.5,"ΠΑΚ",1,"Simatic",0.106,1]
["6ES75901AB600AA0","SIMATIC S7-1500, MOUNTING RAIL 160 MM (APPR. 6.3 INCH); INCL. GROUNDING ELEMENT, INTEGRATED DIN RAIL FOR MOUNTING OF SMALL COMPONENTS SUCH AS CLAMPS, FUSES OR RELAYS",19.3,"TEM",1,"Simatic",0.36799999999999999,0]
["6ES75901AC400AA0","SIMATIC S7-1500, MOUNTING RAIL 245 MM (APPR. 9.6 INCH); INCL. GROUNDING ELEMENT, INTEGRATED DIN RAIL FOR MOUNTING OF SMALL COMPONENTS SUCH AS CLAMPS, FUSES OR RELAYS",32.200000000000003,"TEM",1,"Simatic",0.55400000000000005,0]
["6ES75901AE800AA0","SIMATIC S7-1500, MOUNTING RAIL 482 MM (APPR. 19 INCH) INCL. GROUNDING ELEMENT, INTEGRATED DIN RAIL FOR MOUNTING OF SMALL COMPONENTS SUCH AS CLAMPS, FUSES OR RELAYS",29,"TEM",1,"Simatic",1.038,0]
["6ES75901AF300AA0","SIMATIC S7-1500, MOUNTING RAIL 530 MM (APPR. 20.9 INCH); INCL. GROUNDING ELEMENT, INTEGRATED DIN RAIL FOR MOUNTING OF SMALL COMPONENTS SUCH AS CLAMPS, FUSES OR RELAYS",35.4,"TEM",1,"Simatic",1.151,0]
["6ES75901AJ300AA0","SIMATIC S7-1500, MOUNTING RAIL 830 MM (APPR. 32,7 INCH); INCL. GROUNDING ELEMENT, INTEGRATED DIN RAIL FOR MOUNTING OF SMALL COMPONENTS SUCH AS CLAMPS, FUSES OR RELAYS",46.1,"TEM",1,"Simatic",1.78,0]
["6ES75901BC000AA0","SIMATIC S7-1500, MOUNTING RAIL 2000 MM (APPR. 78.7 INCH); W/O GROUNDING ELEMENT, INTEGRATED DIN RAIL FOR MOUNTING OF SMALL COMPONENTS SUCH AS CLAMPS, FUSES OR RELAYS FOR SELF CONFIGURING, GROUNDING ELEMENT (6ES7590-5AA00-0AA0, 20 PIECES) MUST BE ORDERED SEPARTELY",78.300000000000011,"TEM",1,"Simatic",4.34,0]
["6ES75905AA000AA0","SIMATIC S7, 1500, GROUNDING ELEMENT FOR CONNECTING PE TO THE S7-1500 MOUNTING RAIL; OBLIGATORY FOR THE 2000 MM MOUNTING RAIL 20 PIECES PER PACKAGING UNIT",20.400000000000002,"ΠΑΚ",1,"Simatic",0.33900000000000002,1]
["6ES75905BA000AA0","SIMATIC S7-1500, SPARE PART SHIELDING TERMINAL APPLICABLE FOR ANALOG MODULES AND TECHNOLOGY MODULES W/O SHILDING FRAME AND W/O DC 24V FEEDING ELEMENTS 10 PIECES PER PACKAGING UNIT",31.1,"ΠΑΚ",1,"Simatic",0.255,1]
["6ES75905CA000AA0","SIMATIC S7-1500, SPARE PART SHIELDING SET SET CONSISTS OF * SHIELDING TERMINAL * SHIELDING FRAME * FEEDING ELEMENT DC24V SCREW TYPE, APPLICABLE FOR ANALOG MODULES AND TECHNOLOGY MODULES SUITABLE FOR ALL FRONT CONNECTORS F. 35MM WIDE MODULES 5 PIECES PER PACKAGING UNIT",52.5,"ΠΑΚ",1,"Simatic",0.313,1]
["6ES75905CA100XA0","SIMATIC S7-1500, SPARE PART SHIELDING SET SET CONSISTS OF * 4X SHIELDING TERMINAL * 4X SHIELDING FRAME * 4X FEEDING ELEMENT DC24V PUSH-IN TERMINALS, APPLICABLE FOR S7-1500 ANALOG MODULES, TECHNOLOGY MODULES AND COMPACT CPU, SUITABLE FOR ALL FRONT CONNECTORS F. 25MM WIDE MODULES",42.900000000000006,"TEM",1,"Simatic",0.21199999999999999,1]
["6ES75908AA000AA0","SIMATIC S7-1500 SPARE PART, CONNECTOR PLUG FOR SYSTEM POWER SUPPLY MODULE (PS) AND POWER MODULE (PM) 10 PIECES PER PACKAGING UNIT",108,"ΠΑΚ",1,"Simatic",0.28399999999999997,1]
["6ES75911AA000AA0","SIMATIC S7-1500, SPARE PART DISPLAY FOR CPU 1511-1 PN AND CPU 1513-1 PN",108,"TEM",1,"Simatic",8.7999999999999995E-2,1]
["6ES75911AA010AA0","SIMATIC S7-1500, SPARE PART DISPLAY FOR CPU 1511-1 PN, CPU 1511F-1 PN, CPU 1511C-1 PN, CPU 1512C-1 PN, CPU 1513-1 PN AND CPU 1513F-1 PN",105,"TEM",1,"Simatic",8.7999999999999995E-2,1]
["6ES75911BA000AA0","SIMATIC S7-1500, SPARE PART DISPLAY FORCPU 1515-2 PN, CPU 1516-3 PN/DP, CPU 1517-3 PN/DP AND CPU 1518-4 PN/DP",134,"TEM",1,"Simatic",0.14799999999999999,1]
["6ES75911BA010AA0","SIMATIC S7-1500, SPARE PART DISPLAY FOR CPU 1515(F)-2 PN, CPU 1516(F)-3 PN/DP, CPU 1517(F)-3 PN/DP AND CPU 1518(F)-4 PN/DP",132,"TEM",1,"Simatic",0.14799999999999999,1]
["6ES75913AA000AA0","SIMATIC ET 200SP, SPARE PART 5 FRONT COVERS FOR BUSADAPTER INTERFACE OF ET200SP CPU",25.8,"TEM",1,"Simatic",2.1000000000000001E-2,1]
["6ES75918AA000AA0","SIMATIC S7-1500 SPARE PART, FRONT COVER FOR DP-INTERFACE OF CPU 1518-4 PN/DP",7.5,"TEM",1,"Simatic",0.158,1]
["6ES75921AM000XB0","SIMATIC S7-1500, FRONTCONNECTOR SCREW-TYPE, 40PIN, FOR 35MM WIDE MODULES, INCL. 4 JUMPERS, AND CABLE STRAP",35.4,"TEM",1,"Simatic",0.14199999999999999,1]
["6ES75921AX000AA0","SIMATIC S7-1500, LABELING SHEETS FOR 25MM WIDE S7-1500 MODULES, AND COMPACT CPU, COLOR: AL GREY; MATERIAL: MEMBRANE, PERFORATED, CAN BE USED WITH STANDARD LASER PRINTERS; 10 SHEETS WITH 20 LABELS EACH PER PACKAGING UNIT SUFFICIENT FOR 200 MODULES",51.5,"ΠΑΚ",1,"Simatic",0.218,0]
["6ES75921BM000XA0","SIMATIC S7-1500, FRONTCONNECTOR PUSH-IN TYPE; 40PIN, FOR 25MM WIDE S7-1500 MODULES AND COMPACT CPU, INCL. CABLE STRAP",35.4,"TEM",1,"Simatic",6.7000000000000004E-2,1]
["6ES75921BM000XB0","SIMATIC S7-1500, FRONTCONNECTOR PUSH-IN TYPE, 40PIN, FOR 35MM WIDE MODULES INCL. 4 JUMPERS AND CABLE STRAP",35.4,"TEM",1,"Simatic",0.151,1]
["6ES75922AX000AA0","SIMATIC S7-1500, LABELING SHEETS FOR 35MM WIDE S7-1500 MODULES COLOR: AL GREY MATERIAL: MEMBRANE, PERFORATED; CAN BE USED WITH STANDARD LASER PRINTERS; 10 SHEETS WITH 10 LABELS EACH PER PACKAGING UNIT SUFFICIENT FOR 100 MODULES",51.5,"ΠΑΚ",1,"Simatic",0.22700000000000001,0]
["6ES75922CX000AA0","SIMATIC S7-1500, LABELING SHEETS FOR 35MM WIDE S7-1500 MODULES COLOR: YELLOW, MATERIAL: MEMBRANE, PERFORATED; CAN BE USED WITH STANDARD LASER PRINTERS; 10 SHEETS WITH 10 LABELS EACH PER PACKAGING UNIT SUFFICIENT FOR 100 MODULES",51.5,"TEM",1,"Simatic",0.22700000000000001,0]
["6ES75923AA000AA0","SIMATIC S7-1500, SPARE PART JUMPERS FOR FRONT CONNECTORS FOR 35MM WIDTH IO-MODULES; CAN BE USED FOR ALL DC24V MODULES; 20 PIECES PER PACKAGING UNIT NOTE: MUST NOT BE USED FOR 230V, MUSTNOT BE USED FOR ANALOG MODULES",10.8,"ΠΑΚ",1,"Simatic",8.0000000000000002E-3,0]
["6ES75926EF001AA0","SIMATIC DP, SPARE PART 5 E-CODING ELEMENTS TYPE F, USABLE FOR ET 200MP MODULES F-DI, F-DQ; 5 PIECES PER PACKAGING UNIT",82.5,"ΠΑΚ",1,"Simatic",8.9999999999999993E-3,1]
["6ES76710RC080YA0","SIMATIC WINAC RTX 2010, SINGLE LICENSE F. 1 INSTALL., R-SW, SW AND DOCU. ON DVD, LICENSE KEY ON USB STICK, CLASS A, 3 LANGUAGES (G,E,F), EXECUTABLE UNDER WINDOWS XP SP2, SP3 OR WINDOWS 7 32 BIT, INCL. INTERVALZERO RTX, REFERENCE-HW: SIMATIC PC",1399,"TEM",1,"Simatic",0.22700000000000001,0]
["6ES76710RC080YE0","SIMATIC WINAC RTX 2010 UPGRADE UPGRADE F. WINAC BASIS/RTX VERSIONS V3.X, V4.X, 200X. SINGLE LICENSE FOR 1 INSTALL., R-SW, SW AND DOCU. ON CD, LICENSE KEY ON USB STICK, CLASS A, 3 LANGUAGES (G,E,F), EXECUTABLE UNDER WINDOWS XP SP2, SP3 OR WINDOWS 7 32 BIT, INCL. INTERVALZERO RTX, REFERENCE-HW: SIMATIC PC",512,"TEM",1,"Simatic",0.22500000000000001,0]
["6ES76710RC080YU8","SIMATIC WINAC RTX 2010, UPDATE DVD FOR SP2 R-SW, SW AND DOCU. ON DVD WITHOUT LICENSE ONLY TO BE USED WITH EXISTING WINAC RTX 2010 LICENSE",55.7,"TEM",1,"Simatic",0.218,0]
["6ES76710RC086YA0","SIMATIC WINAC RTX 2010 PACKAGE, SW PACKAGE FOR SIMATIC IPC CONSISTING OF: SIMATIC WINAC RTX 2010 AVAILABLE ONLY W. SAME QTY OF SIMATIC IPC ON SAME ORDER FORM",1045,"TEM",1,"Simatic",0.23599999999999999,0]
["6ES76710XY004AB0","SIMATIC WINAC SIBAS PN RTX V1.0 CUSTOER SPECIFIC CONTROL SW FORSIBAS SYSTEMS LICENSE ONLY (COL)",433,"TEM",1,"Simatic",0.05,0]
["6ES76711RC080YA0","SIMATIC WINAC RTX F 2010, SINGLE LICENSE F. 1 INSTALL., R-SW, SW AND DOCU. ON DVD, LICENSE KEY ON USB STICK, CLASS A, 2 LANGUAGES (G,E), EXECUTABLE UNDER WINDOWS XP SP2, SP3 OR WINDOWS 7 32 BIT, INCL. INTERVALZERO RTX, REFERENCE-HW: SIMATIC PC",2713,"TEM",1,"Simatic",0.23200000000000001,0]
["6ES76711RC080YE0","SIMATIC WINAC RTX F 2010 UPGR UPGRADE F. WINAC RTX F VERSION 2009, SINGLE LICENSE FOR 1 INSTALL., R-SW, SW AND DOCU. ON CD, LICENSE KEY ON USB STICK, CLASS A, 2 LANGUAGES (G,E), EXECUTABLE UNDER WINDOWS XP SP2, SP3 OR WINDOWS 7 32 BIT, INCL. INTERVALZERO RTX, REFERENCE-HW: SIMATIC PC",953,"TEM",1,"Simatic",0.224,0]
["6ES76711RC080YS0","TRAINING BUNDLE WINAC RTX F 2010 / CP 5622 CONSISTING OF: 1 X SIMATIC WINAC RTX F 2010, SINGLE LICENSE F. 1 INSTALL., R-SW, SW AND DOCU. ON CD, LICENSE KEY ON USB STICK, CLASS A, 2LANGUAGES (G, E), EXECUTABLE UNDER WINXP SP2/SP3 ODER WIN7 32BIT, INCL. INTERVALZERO RTX, REFERENCE HW: SIMATIC PC 1 X COMMUNICATION PROC. CP5622 PCI EXPRESS X1-CARD (32 BIT); FOR CONNECT. A PG OR A PC WITH PCI EXPRESS-BUS TO PROFIBUS OR MPI; ******************************* FOR EDUCATIONAL PURPOSES ONLY",1223,"TEM",1,"Simatic",0.8,0]
["6ES76711RC080YU8","SIMATIC WINAC RTX F 2010, UPDATE DVD FOR SP2 R-SW, SW AND DOCU. ON DVD WITHOUT LICENSE ONLY TO BE USED WITH EXISTING WINAC RTX 2010 LICENSE",55.800000000000004,"TEM",1,"Simatic",0.215,0]
["6ES76711RC086YA0","SIMATIC WINACRTX F 2010 PACKAGE SW PACKAGE FOR SIMATIC IPC CONSISTING OF: SIMATIC WINAC RTX F 2010 AVAILABLE ONLY WITH SAME QTY OF SIMATIC IPC ON SAME ORDER FORM",1428,"TEM",1,"Simatic",0.1,0]
["6ES76711RC185YB0","SIMATIC WINAC RTX F 2010 OEM, UNLOCK COPY LICENSE, ADDITIONAL PACKAGE FOR 10 INSTALLATIONS, ONLY VALID COMBINED WITH UNLOCK COPY LIVENSE CONTRACT, REQUIRES UCL BASIC PACKAGE COL STICKER",27124,"TEM",1,"Simatic",0.1,0]
["6ES76725DC010YK0","SIMATIC S7-1500 software controller CPU 1505SP, version 2.0 upgrade, upgrade for CPU 1505S V1.X on ET 200SP open controller, Single License f. 1 InSTall., R-SW, software, docu and license key download, R-SW, class A, 6 languages (Ge,En,It,Fr,Sp,Cn) ******************************* Email address is mandatory for delivery!",273,"TEM",1,"Simatic",1E-3,0]
["6ES76727AC010YA0","SIMATIC S7-1500, Software controller CPU 1507S Version 2.0, Single license f. 1 inSTall., R-SW, sw and docu. on DVD, license key on USB STick, RT-SW class A, 6 languages (Ge,En,It,Fr,Sp,Cn) executable under Windows 7 reference HW: SIMATIC IPC2x7E, IPC4x7D, IPC6x7D, IPC8x7D",1024,"TEM",1,"Simatic",0.2,0]
["6ES76727AC010YG0","SIMATIC S7-1500, Software Controller CPU 1507S Version 2.0, Single License f. 1 InSTall., R-SW, software, doku. and license key download, RT-SW class A, 6 languages (Ge,En,It,Fr,Sp,Cn) executable under Windows 7 reference HW: SIMATIC IPC2x7E, IPC4x7D, IPC6x7D, IPC8x7D ******************************* Email address is mandatory for delivery!",977,"TEM",1,"Simatic",1E-3,0]
["6ES76727AC010YK0","SIMATIC S7-1500, Software Controller CPU 1507S Version 2.0 upgrade, upgrade for CPU 1507S V1.8, Single License f. 1 InSTall., R-SW, software, doku. and license key download, RT-SW class A, 6 languages (Ge,En,It,Fr,Sp,Cn) executable under Windows 7 reference HW: SIMATIC IPC2x7E, IPC4x7D, IPC6x7D, IPC8x7D ******************************* Email address is mandatory for delivery!",391,"TEM",1,"Simatic",1E-3,0]
["6ES76727FC010YA0","SIMATIC S7-1500 Fail-safe Software controllerCPU 1507S F Version 2.0, Single license f. 1 inSTall., R-SW, sw and docu. on DVD, license key on USB STick, RT-SW class A, 6 languages (Ge,En,It,Fr,Sp,Cn) executable under Windows 7 reference HW: SIMATIC IPC2x7E and IPC4x7D",1357,"TEM",1,"Simatic",0.2,0]
["6ES76727FC010YG0","SIMATIC S7-1500 Failsafe Software Controller CPU 1507S F Version 2.0, Single License f. 1 InSTall., R-SW, software, doku. and license key download, RT-SW class A, 6 languages (Ge,En,It,Fr,Sp,Cn) executable under Windows 7 reference HW: SIMATIC IPC2x7E and IPC4x7D ******************************* Email address is mandatory for delivery!",1292,"TEM",1,"Simatic",1E-3,0]
["6ES76771FD004AB1","TRAINING BUNDLE  S7-MEC EC31-RTX F, CONSISTING OF: EC31-RTX F, EM PCI-104 EXTENSION MODULE EM PC EXTENSION MODULE RAIL 2000MM, POWER SUPPLY PS 307 10A, 1 X SM323 16DI/16DO, 1 X SM334 4AI/ 2AO, SM374 SIMULATOR MODULE, SIMATIC WINAC ODK V4.2, S7 DISTRIBUTED SAFETY V5.4 ******************************* FOR EDUCATIONAL PURPOSES ONLY",3147,"TEM",1,"Simatic",8,0]
["6ES76772AA310EB0","SIMATIC ET 200SP OPEN CONTROLLER, CPU 1515SP PC, 4 GB RAM, 8 GB CFAST WITH WINDOWS EMBEDDED STANDARD 7 E 32BIT PREINSTALLED, W. S7-1500 SOFTWARE CONTROLLER CPU 1505S V1.8 PREINSTALLED, INTERFACES: 1X SLOT CFAST, 1X SLOT SD/MMC, 1X PLUG F. ET 200SP BUS- ADAPTOR PROFINET, 1X 10/100/1000 MBIT/S ETHERNET, 3 X USB, 1 X DVI-I GRAPHIC INTERFACE, DOCUMENTATION ON DVD, RESTORE DVD",2027,"TEM",1,"Simatic",1.075,0]
["6ES76772AA400AA0","SIMATIC ET 200SP OPEN CONTROLLER, CPU 1515SP PC, SPARE PART, 4 GB RAM, WITHOUT CFAST INTERFACES: 1X SLOT CFAST, 1X SLOT SD/MMC, 1X PLUG F. ET 200SP BUS- ADAPTOR PROFINET, 1X 10/100/1000 MBIT/S ETHERNET 3 X USB, 1 X DVI-I GRAPHIC INTERFACE",1733,"TEM",1,"Simatic",0.83,1]
["6ES76772AA410FB0","SIMATIC ET 200SP OPEN CONTROLLER, CPU 1515SP PC, 4 GB RAM, 16 GB CFAST WITH WINDOWS EMBEDDED STANDARD 7 P 64BIT PREINSTALLED, W. S7-1500 SOFTWARE CONTROLLER CPU 1505S V1.8 PREINSTALLED, INTERFACES: 1X SLOT CFAST, 1X SLOT SD/MMC, 1X PLUG F. ET 200SP BUS- ADAPTOR PROFINET, 1X 10/100/1000 MBIT/S ETHERNET, 3 X USB, 1 X DVI-I GRAPHIC INTERFACE, DOCUMENTATION ON DVD, RESTORE DVD",2363,"TEM",1,"Simatic",0.83,0]
["6ES76772AA410FK0","SIMATIC ET 200SP OPEN CONTROLLER, CPU 1515SP PC + HMI 128PT, 4 GB RAM, 16 GB CFAST WITH WINDOWS EMBEDDED STANDARD 7 P 64BIT PREINSTALLED, W. S7-1500 SOFTWARE CONTROLLER CPU 1505S V1.8 PREINSTALLED, WITH WINCC RUNTIME ADVANCED V13 SP1 PREINSTALLED WITH 128 POWERTAGS LICENSE, INTERFACES: 1X SLOT CFAST, 1X SLOT SD/MMC, 1X PLUG F. ET 200SP BUS- ADAPTOR PROFINET, 1X 10/100/1000 MBIT/S ETHERNET, 3 X USB, 1 X DVI-I GRAPHIC INTERFACE, DOCUMENTATION ON DVD, RESTORE DVD",2646,"TEM",1,"Simatic",0.83,0]
["6ES76772AA410FL0","SIMATIC ET 200SP OPEN CONTROLLER, CPU 1515SP PC + HMI 512PT, 4 GB RAM, 16 GB CFAST WITH WINDOWS EMBEDDED STANDARD 7 P 64BIT PREINSTALLED, W. S7-1500 SOFTWARE CONTROLLER CPU 1505S V1.8 PREINSTALLED, WITH WINCC RUNTIME ADVANCED V13 SP1 PREINSTALLED WITH 512 POWERTAGS LICENSE, INTERFACES: 1X SLOT CFAST, 1X SLOT SD/MMC, 1X PLUG F. ET 200SP BUS- ADAPTOR PROFINET, 1X 10/100/1000 MBIT/S ETHERNET, 3 X USB, 1 X DVI-I GRAPHIC INTERFACE, DOCUMENTATION ON DVD, RESTORE DVD",3255,"TEM",1,"Simatic",0.83,0]
["6ES76772AA410FM0","SIMATIC ET 200SP OPEN CONTROLLER, CPU 1515SP PC + HMI 2048PT, 4 GB RAM, 16 GB CFAST WITH WINDOWS EMBEDDED STANDARD 7 P 64BIT PREINSTALLED, W. S7-1500 SOFTWARE CONTROLLER CPU 1505S V1.8 PREINSTALLED, WITH WINCC RUNTIME ADVANCED V13 SP1 PREINSTALLED WITH 2048 POWERTAGS LICENSE, INTERFACES: 1X SLOT CFAST, 1X SLOT SD/MMC, 1X PLUG F. ET 200SP BUS- ADAPTOR PROFINET, 1X 10/100/1000 MBIT/S ETHERNET, 3 X USB, 1 X DVI-I GRAPHIC INTERFACE, DOCUMENTATION ON DVD, RESTORE DVD",3733,"TEM",1,"Simatic",0.83,0]
["6ES76772AA414AB1","TRAINING BUNDLE CPU 1515SP PC + HMI 512PT CONSISTING OF: CPU 1515SP PC + HMI 512PT, 4GB RAM, 16GB CFAST W. WES7 P, S7-1500 SW-CONTROLLER INSTALL., WINCC RT ADV. 512PT INSTALL., SIMATIC ODK 1500S, 1X BUSADAPTER BA 2XRJ45, 16 DI, 16 DQ, 4X BASEUNITS, ETHERNET CORD RJ45/RJ45 6M, MOUNTING RAIL, 483 MM, LABELING STRIPS, COLOUR CODED LABELS ******************************* FOR EDUCATIONAL PURPOSES ONLY",1922,"TEM",1,"Simatic",3,0]
["6ES77170BB008AB0","SIMATIC FIELD PG M5 COMFORT FOR INTERNAL USE ONLY (ZN/LG); I5-6440EQ (2.7 UP TO 3.4 GHZ; 4 CORES, 6M SMART CACHE); 15.6\" DISPLAY, FULL HD; WLAN 802.11AC & BLUETOOTH V4.0; DVD +/-RW; HD GRAPHICS 530; 1X 16GB DDR4 SDRAM SO-DIMM; 512 GB SSD SATA (2.5\"); W/O S5-INTERFACE, W/O S5-EPROMMER; POWER CORD WITH POWER PLUG: EUROPE; KEYBOARD: QWERTZ / QWERTY; WINDOWS 7 ULTIMATE SP1, 64-BIT; LICENSE FOR STEP7 PROF V13; WINCC ADVANCED V13; VERSION OF SOFTWARE  V13.0.1.0:",6148,"TEM",1,"Simatic",3.5,0]
["6ES77171CC008AB0","SIMATIC FIELD PG M5 ADVANCED FOR INTERNAL USE ONLY (ZN/LG); I7-6820EQ (2.8 UP TO 3.5 GHZ; 4 CORES + HYPER-THREADING; 8 MB SMART CACHE); 15.6\" DISPLAY, FULL HD; WLAN 802.11AC & BLUETOOTH V4.0; DVD +/-RW; HD GRAPHICS 530; 2X 16GB DDR4 SDRAM SO-DIMM; 1 TB SSD SATA (2.5\"); W/O S5-INTERFACE, W/O S5-EPROMMER; POWER CORD WITH POWER PLUG: EUROPE; KEYBOARD: QWERTZ / QWERTY; WINDOWS 7 ULTIMATE SP1, 64-BIT; LICENSE FOR STEP7 PROF V13; WINCC ADVANCED V13; VERSION OF SOFTWARE  V13.0.1.0:",7686,"TEM",1,"Simatic",3.5,0]
["6ES77901AA010AA0","SIMATIC FIELD PG ACCESSORIES USB 3.0 - SATA - ADAPTER FOR HARDDRIVE KIT 6ES7791-2BA01-0AA0 6ES7791-2BA20-0AA0 FOR FIELD PG M5/M4/M3",68.3,"TEM",1,"Simatic",0.104,0]
["6ES77912BA020AA0","SIMATIC FIELD PG M5/M4 HARDDRIVE-KIT 1 TB SATA INCL. BAG AND SCREW DRIVER FOR FIELD PG M5/M4 ONLY",237,"TEM",1,"Simatic",0.42099999999999999,0]
["6ES77912BA220AA0","SIMATIC Field PG M5 Solid STate DriveE Kit, 512 GB SATA SSD incl. bag and screwdriver for Field PG M5",588,"TEM",1,"Simatic",0.38300000000000001,0]
["6ES77912BA230AA0","SIMATIC Field PG M5 Solid STate DriveE Kit, 1 TB SATA SSD incl. bag and screwdriver for Field PG M5",1050,"TEM",1,"Simatic",0.38500000000000001,0]
["6ES77926WA011YA0","SIMATIC FIELD PG M3 OPERATING SYSTEM PACKAGE, MICROSOFT WINDOWS 7 ULTIMATE SP1 X64 FOR FIELD PG M3",368,"TEM",1,"Simatic",0.20399999999999999,0]
["6ES77926WA012YA0","SIMATIC FIELD PG M4 OPERATING SYSTEM PACKAGE, MICROSOFT WINDOWS 7 ULTIMATE SP1 X64 FOR FIELD PG M4",368,"TEM",1,"Simatic",0.93799999999999994,0]
["6ES77980AA080XA0","SIMATIC PG, spare battery lithium-ion 8.8 Ah, for Field PG M5, warranty: 6 months",200,"TEM",1,"Simatic",0.55900000000000005,1]
["6ES77980CA000XA0","SIMATIC PG,  ADAPTER FOR S5 EPROM PROGRAMMING IN THE FIELD PG AND POWER PG",189,"TEM",1,"Simatic",5.5E-2,1]
["6ES77980DA020XA0","SIMATIC PG, BACKPACK FOR FIELD PG M5/M4 IN THE SCOPE OF SUPPLY OF FIELD MG M5",68.3,"TEM",1,"Simatic",0.85,1]
["6ES77980GA040XA0","SIMATIC PG,  AC/DC power supply for Field PG M5 w/o power cable",84,"TEM",1,"Simatic",0.58899999999999997,1]
["6ES78030CA010YX2","SIMATIC S7, DOCPRO SOFTWARE UPDATE SERVICE WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE",179,"TEM",1,"Simatic",0.3,0]
["6ES78030CC002YX0","SIMATIC S7, DOCPRO EPL-MASTER, ROYALTY-DUTY PER 1 INSTALLATION, ONLY VALID COMBINED W. ENTERPRISE LICENSE CONTRACT, E-SW, SW AND DOCU. ON CD, LICENSE KEY ON CD/FD; CLASS A",360,"TEM",1,"Simatic",0.4,0]
["6ES78030CC002YX1","SIMATIC S7, DOCPRO EPL-ROYALTY, SINGLE LICENSE F.1 INSTALLATION E-SW, WITHOUT SW AND DOCU., CLASS A, ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",861,"TEM",1,"Simatic",0.1,0]
["6ES78030CC002YX2","SIMATIC S7, DOCPRO EPL-MAINTENANCE, MAINTENANCE CHARGE F. ROYALTY FOR 12 MONTHS, ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",179,"TEM",1,"Simatic",0.1,0]
["6ES78030CC030YA5","SIMATIC S7, DOCPRO V5.4 FLOATING LICENSE F.1 USER E-SW, SW AND DOCU. ON CD, LICENSE KEY ON USB STICK, CLASS A, 5 LANGUAGES (G,E,F,I,S), EXECUTABLE UNDER WINXPPROF, WIN 7 ULTIMATE/PROF, REFERENCE-HW:PG/PC",861,"TEM",1,"Simatic",0.23,0]
["6ES78030CC030YE5","SIMATIC S7, DOCPRO V5.4 UPGRADE, FLOATING LICENSE FOR 1 USER E-SW, SW AND DOCU. ON CD LICENSE KEY ON USB STICK, CLASS A, 5 LANGUAGES (G,E,F,I,S), EXECUTABLE UNDER WINXPPROF, WIN 7 ULTIMATE/PROF,",300,"TEM",1,"Simatic",0.253,0]
["6ES78030CC032YN8","SIMATIC S7, DOCPRO V5.4 UNLOCK COPY LICENSE, ONLY VALID COMBINED W. UNLOCK COPY LICENSE CONTRACT AND VALID LICENSE",360,"TEM",1,"Simatic",0.1,0]
["6ES78061CC030BA0","SIMATIC WINAC ODK V4.2, SINGLE LICENSE F. 1 INSTALL., E-SW, SW AND DOCU. ON CD, CLASS A, 1 LANGUAGE (E), EXECUTABLE UNDER WINDOWS XP SP2, SP3 OR WINDOWS 7 32 BIT REFERENCE-HW: SIMATIC PC",1364,"TEM",1,"Simatic",0.20399999999999999,0]
["6ES78062CD020YA0","SIMATIC ODK 1500S V2.0 Single License f. 1 InSTall., E-SW, sw and docu. on DVD, class A, 2 languages (Ge, En), executable under Windows 7, Windows 8.1 and Windows 10",2888,"TEM",1,"Simatic",0.2,0]
["6ES78062CD020YG0","SIMATIC ODK 1500S V2.0 Single License f. 1 InSTall., E-SW, sw and docu. download, class A, 2 languages (Ge, En), executable under Windows 7, Windows 8.1 and Windows 10 ******************************* Email address is mandatory for delivery!",2625,"TEM",1,"Simatic",1E-3,0]
["6ES78073BA010YA0","SIMATIC S7,PRODAVE MPI MINIV6.0 SINGLE LICENSE F.1 INSTALLATION R-SW, SW AND DOCU. ON CD, CLASS A, 2 LANGUAGES (G,E), EXECUTABLE UNDER WIN98/ME/ WINNT/2000PROF/XP, REFERENCE-HW:PG/PC",236,"TEM",1,"Simatic",0.222,0]
["6ES78073BA010YA1","SIMATIC S7,PRODAVE MPI MINIV6.0 SINGLE LICENSE F.1 INSTALLATION R-SW, WITHOUT SW AND DOCU., CLASS A, 2 LANGUAGES (G,E), EXECUTABLE UNDER WIN98/ME/ WINNT/2000PROF/XP, REFERENCE-HW:PG/PC",168,"TEM",1,"Simatic",0.22,0]
["6ES78074BA030YA0","SIMATIC S7, PRODAVE MPI/IE V6.2 SINGLE LICENSE F.1 INSTALLATION R-SW, SW AND DOCU. ON CD, CLASS A, 2 LANGUAGES (G,E), EXECUTABLE UNDER WINXPPROF, WINDOWS 7 ULTIM./PRO 32/64BIT REFERENCE-HW:PG/PC",605,"TEM",1,"Simatic",0.216,0]
["6ES78074BA030YA1","SIMATIC S7, PRODAVE MPI/IE V6.2 COPY LICENSE F.1 INSTALLATION R-SW, SW AND DOCU. ON CD, CLASS A, 2 LANGUAGES (G,E), EXECUTABLE UNDER WINXPPROF, WINDOWS 7 ULTIM./PRO 32/64BIT REFERENCE-HW:PG/PC",455,"TEM",1,"Simatic",0.224,0]
["6ES78104BC010YX2","SIMATIC S7, STEP7 SOFTWARE UPDATE SERVICE WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE",347,"TEM",1,"Simatic",0.3,0]
["6ES78104CA108AW0","SIMATIC S7, STEP7 DOCUMENTATION BASIC KNOWLEDGE, COMPRISES: GETTING STARTED,HW-CONFIG-MAN., PROGRAMM. MANUAL, S5 CONVERTER MAN. FOR V5.5, GERMAN",168,"TEM",1,"Simatic",7.5,0]
["6ES78104CA108AW1","SIMATIC S7, STEP7 DOCUMENTATION REFERENCE MANUAL, COMPRISES: MANUAL FOR STL/LAD/CSF REFERENCE MANUAL S7-300/400 FOR V5.5, GERMAN",168,"TEM",1,"Simatic",7.5,0]
["6ES78104CA108BW0","SIMATIC S7, STEP7 DOCUMENTATION BASIC KNOWLEDGE, COMPRISES: GETTING STARTED,HW-CONFIG-MAN., PROGRAMM. MANUAL,S-5 CONVERTER MAN. FOR V5.5, ENGLISH",168,"TEM",1,"Simatic",3.6309999999999998,0]
["6ES78104CA108BW1","SIMATIC S7, STEP7 DOCUMENTATION REFERENCE MANUAL, COMPRISES: MANUAL FOR STL/LAD/CSF REFERENCE MANUAL S7-300/400 FOR V5.5, ENGLISH",168,"TEM",1,"Simatic",3.8330000000000002,0]
["6ES78104CA108CW0","SIMATIC S7, STEP7 DOCUMENTATION BASIC KNOWLEDGE, COMPRISES: GETTING STARTED,HW-CONFIG-MAN., PROGRAMM. MANUAL,S-5 CONVERTER MAN. FOR V5.5, FRENCH",168,"TEM",1,"Simatic",3.8559999999999999,0]
["6ES78104CA108CW1","SIMATIC S7, STEP7 DOCUMENTATION REFERENCE MANUAL, COMPRISES: MANUAL FOR STL/LAD/CSF REFERENCE MANUAL S7-300/400 FOR V5.5, FRENCH",168,"TEM",1,"Simatic",4.0739999999999998,0]
["6ES78104CA108DW0","SIMATIC S7, STEP7 DOCUMENTATION BASIC KNOWLEDGE, COMPRISES: GETTING STARTED,HW-CONFIG-MAN., PROGRAMM. MANUAL,S-5 CONVERTER MAN. FOR V5.5, SPANISH",168,"TEM",1,"Simatic",3.7669999999999999,0]
["6ES78104CA108DW1","SIMATIC S7, STEP7 DOCUMENTATION REFERENCE MANUAL, COMPRISES: MANUAL FOR STL/LAD/CSF REFERENCE MANUAL S7-300/400 FOR V5.5, SPANISH",168,"TEM",1,"Simatic",3.9660000000000002,0]
["6ES78104CA108EW0","SIMATIC S7, STEP7 DOCUMENTATION BASIC KNOWLEDGE, COMPRISES: GETTING STARTED,HW-CONFIG-MAN., PROGRAMM. MANUAL,S-5 CONVERTER MAN. FOR V5.5, ITALIAN",168,"TEM",1,"Simatic",3.7959999999999998,0]
["6ES78104CA108EW1","SIMATIC S7, STEP7 DOCUMENTATION REFERENCE MANUAL, COMPRISES: MANUAL FOR STL/LAD/CSF REFERENCE MANUAL S7-300/400 FOR V5.5, ITALIAN",168,"TEM",1,"Simatic",7.5,0]
["6ES78104CC002YX0","SIMATIC S7, STEP7 EPL-MASTER, ROYALTY-DUTY PER 1 INSTALLATION, ONLY VALID COMBINED W. ENTERPRISE LICENSE CONTRACT, E-SW, SW AND DOCU. ON CD, LICENSE KEY ON CD/FD; CLASS A",330,"TEM",1,"Simatic",0.25,0]
["6ES78104CC002YX1","SIMATIC S7, STEP7 EPL-ROYALTY, SINGLE LICENSE F.1 INSTALLATION E-SW, WITHOUT SW AND DOCU., CLASS A, ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",1890,"TEM",1,"Simatic",1E-3,0]
["6ES78104CC002YX2","SIMATIC S7, STEP7 EPL-MAINTENANCE, MAINTENANCE CHARGE F. ROYALTY FOR 12 MONTHS, ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",347,"TEM",1,"Simatic",1E-3,0]
["6ES78104CC100JA5","SIMATIC S7, STEP7 V5.5 JAPANESE FLOATING LICENSE F.1 USER E-SW, SW AND DOCU. ON DVD, LICENSE KEY ON USB STICK CLASS A, 2 LANGUAGES (E,J), EXECUTABLE UNDER WIN XP PROF JAPANESE, WIN 7 ULTIMATE JAPANESE, WIN 7 PROFESSIONAL JAPANESE REFERENCE-HW: S7-300/400, C7",1890,"TEM",1,"Simatic",0.25,0]
["6ES78104CC100JE5","SIMATIC S7, STEP7 V5.5 JAPANESE UPGRADE, FLOATING LICENSE F.1 USER E-SW, SW AND DOCU. ON DVD, LICENSE KEY ON USB STICK CLASS A, 2 LANGUAGES (E,J), EXECUTABLE UNDER WIN XP PROF JAPANESE, WIN 7 ULTIMATE JAPANESE, WIN 7 PROFESSIONAL JAPANESE REFERENCE-HW: S7-300/400, C7",475,"TEM",1,"Simatic",0.248,0]
["6ES78104CC100KA5","SIMATIC S7, STEP7 V5.5 CHINESE FLOATING LICENSE F.1 USER E-SW, SW AND DOCU. ON DVD, LICENSE KEY ON USB STICK KLASSE A, 2 LANGUAGES (E,C), EXECUTABLE UNDER WIN XP PROF CHINESE, WIN 7 PROF CHINESE, WIN 7 ULTIMATE REFERENCE-HW: S7-300/400, C7",1890,"TEM",1,"Simatic",0.222,0]
["6ES78104CC100KE5","SIMATIC S7, STEP7 V5.5 CHINESE UPGRADE, FLOATING LICENSE F.1 USER E-SW, SW AND DOCU. ON DVD, LICENSE KEY ON USB STICK CLASS A, 2 LANGUAGES (E,C), EXECUTABLE UNDER WIN XP PROF CHINESE, WIN 7 PROF CHINESE, WIN 7 ULTIMATE REFERENCE-HW: S7-300/400, C7",475,"TEM",1,"Simatic",0.22800000000000001,0]
["6ES78104CC100YA5","SIMATIC S7, STEP7 V5.5 SP4, FLOATING LICENSE FOR 1 USER, E-SW, SW AND DOCU. ON DVD, LICENSE KEY ON USB STICK, CLASS A, 5 LANGUAGES (GE,EN,FR,IT,SP), EXECUTABLE UNDER WINXPPROF, WINDOWS 7 ULTIMATE, WINDOWS 7 PROFESSIONAL REFERENCE-HW: S7-300/400, C7",1890,"TEM",1,"Simatic",0.215,0]
["6ES78104CC100YA6","SIMATIC S7, STEP7 V5.5 SP4, DATA MEDIUM INCL. RENTAL LICENSE FOR 50 HOURS, E-SW, SW AND DOCU. ON DVD, LICENSE KEY ON USB STICK, CLASS A, 5 LANGUAGES (GE,EN,FR,IT,SP), EXECUTABLE UNDER WINXPPROF, WINDOWS 7 ULTIMATE, WINDOWS 7 PROFESSIONAL REFERENCE-HW: S7-300/400, C7",336,"TEM",1,"Simatic",0.23400000000000001,0]
["6ES78104CC100YA7","SIMATIC S7, STEP7 V5.5 SP4, DATA MEDIUM INCL. TRIAL LICENSE FOR 14 DAYS, E-SW, SW AND DOCU. ON DVD, LICENSE KEY ON DVD, CLASS A, 5 LANGUAGES (GE,EN,FR,IT,SP), EXECUTABLE UNDER WINXPPROF, WINDOWS 7 ULTIMATE, WINDOWS 7 PROFESSIONAL, REFERENCE-HW: S7-300/400, C7",29,"TEM",1,"Simatic",0.21299999999999999,0]
["6ES78104CC100YE5","SIMATIC S7, STEP7 V5.5 UPGRADE, (V3.X ... V5.4 TO V5.5), FLOATING LICENSE FOR 1 USER, E-SW, SW AND DOCU. ON DVD, LICENSE KEY ON USB STICK, CLASS A, 5 LANGUAGES (GE,EN,FR,IT,SP), EXECUTABLE UNDER WINXPPROF, WINDOWS 7 ULTIMATE, WINDOWS 7 PROFESSIONAL REFERENCE-HW: S7-300/400, C7",475,"TEM",1,"Simatic",0.22,0]
["6ES78104CC102YA0","SIMATIC S7, STEP7 V5.5, UNLOCK COPY LICENSE (UCL), BASIC PACKAGE FOR 20 INSTALLATIONS, ONLY VALID COMBINED WITH UNLOCK COPY LICENSE CONTRACT",22683,"TEM",1,"Simatic",0.26500000000000001,0]
["6ES78104CC102YB0","SIMATIC S7, STEP7 V5.5, UNLOCK COPY LICENSE (UCL), ADDITIONAL PACKAGE FOR 5 INSTALLATIONS, ONLY VALID COMBINED WITH UNLOCK COPY LICENSE CONTRACT, REQUIRES UCL BASIC PACKAGE",5672,"TEM",1,"Simatic",0.05,0]
["6ES78104CC102YE0","SIMATIC S7,STEP7 V5.5 UNLOCK COPY LICENSE (UCL), UCL UPGRADE (V5.4 TO V5.5) FOR 1 INSTALLATION, ONLY VALID COMBINED WITH UNLOCK COPY LICENSE CONTRACT, REQUIRES UCL BASIC PACKAGE MINIMUM ORDER QUANTITY 20 PIECES",285,"TEM",1,"Simatic",0.26500000000000001,0]
["6ES78104CE100YB5","SIMATIC S7, STEP7 V5.5 SP4 FLOATING LICENSE FOR 1 USER E-SW, SW AND DOKU AS DOWNLOAD, LICENSE KEY AS DOWNLOAD, CLASS A, 5 LANGUAGES (GE,EN,FR,IT,SP), EXECUTABLE UNDER WINXPPROF, WINDOWS 7 ULTIMATE, WINDOWS 7 PROFESSIONAL REFERENCE-HW: S7-300/400, C7 ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY!",1748,"TEM",1,"Simatic",1.4999999999999999E-2,0]
["6ES78104CE100YB6","SIMATIC S7, STEP7 V5.5 SP4 RENTAL LICENSE FOR 50 HOURS, E-SW, SW AND DOKU AS DOWNLOAD, LICENSE KEY AS DOWNLOAD, CLASS A, 5 LANGUAGES (GE,EN,FR,IT,SP), EXECUTABLE UNDER WINXPPROF, WINDOWS 7 ULTIMATE WINDOWS 7 PROFESSIONAL REFERENCE-HW: S7-300/400, C7 ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY!",311,"TEM",1,"Simatic",1.4999999999999999E-2,0]
["6ES78105AA002YL0","STEP 7 PROFESSIONAL COMBO INCL. TIA PORTAL, SOFTWARE UPDATE SERVICE F. UCL UNLOCK COPY LICENSE, AUTOMATIC SUPPLY OF UPGRADES AND SERVICE PACKS FOR ONE YEAR WITH AUTOMATIC RENEWAL, REQUIRES LATEST SW VERSION, ONLY VALID COMBINED WITH UNLOCK COPY LICENSE CONTRACT",315,"TEM",1,"Simatic",0.1,0]
["6ES78105CC000YM2","SIMATIC S7 STEP7 PROF COMBO INCL. TIA PORTAL, SOFTWARE UPDATE SERVICE COMPACT WITH MULTIPLE ORDERS FROM ONE IST SUPPLIES WILL BE COMBINED INTO ONE PACKAGE. MINIMUM QUANTITY ORDER: 3 PCS. WITHIN THE FRAMEWORK OF THIS CONTRACT YOU WILL RECEIVE ALL UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. THE CONTRACT WILL BE EXTENDED AUTOMATICALLY BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE. PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE",525,"TEM",1,"Simatic",0.1,0]
["6ES78105CC002YD0","SIMATIC S7, STEP7 PROF 2010 SR4 W/O TIA PORTAL, EPL-POWERPACK, SINGLE LICENSE F.1 INSTALLATION E-SW, WITHOUT SW AND DOCU. CLASS A, ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",1217,"TEM",1,"Simatic",0.05,0]
["6ES78105CC002YE0","SIMATIC S7, STEP7 PROF 2010 SR4/V14, COMBO INCL. TIA PORTAL, EPL-MASTER, ROYALTY-DUTY PER 1 INSTALLATION, REQUIRES LATEST SW-RELEASE ENTERPRISE LICENSE CONTRACT E-SW, SW AND DOCU. ON CD, LICENSE KEY ONF CD/FD; CLASS A",330,"TEM",1,"Simatic",0.3,0]
["6ES78105CC002YE1","SIMATIC S7 STEP7 PROF 2010 SR4/V14, COMBO INCL. TIA PORTAL, EPL-ROYALTY, SINGLE LICENSE F.1 INSTALLATION E-SW, WITHOUT SW AND DOCU. CLASS A, ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",3304,"TEM",1,"Simatic",0.05,0]
["6ES78105CC002YE2","SIMATIC S7 STEP7 PROF 2010 SR4/V14, COMBO INCL. TIA PORTAL, EPL-MAINTENANCE, MAINTENANCE CHARGE F. ROYALTY FOR 12 MONTHS, ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",525,"TEM",1,"Simatic",0.05,0]
["6ES78105CC040YE2","SIMATIC S7 STEP7 PROF COMBO INKL. TIA PORTAL, SOFTWARE UPDATE SERVICE WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE",525,"TEM",1,"Simatic",2.1000000000000001E-2,0]
["6ES78105CC040YY2","SIMATIC STEP7 PROF COMBO SUS DL INCL. TIA PORTAL, SOFTWARE UPDATE SERVICE (SUS) DOWNLOAD, WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY!",515,"TEM",1,"Simatic",1E-3,0]
["6ES78105CC110YA5","SIMATIC S7 STEP7 PROF 2010 SR4/V14 COMBO INCL. TIA PORTAL, FLOATING LICENSE FOR 1 USER, E-SW, SW AND DOCU. ON DVD, LICENSE KEY ON USB STICK , CLASS A, 5/6 LANGUAGES (GE,EN,FR,IT,SP)/(CN), EXECUTABLE UNDER WINDOWS XP FOR 2010 ONLY, WINDOWS 7 FOR 2010 & V14, WINDOWS 8.1 FOR V14 ONLY REFERENCE-HW: S7-300/400 (S7-1200/1500)",3304,"TEM",1,"Simatic",0.66700000000000004,0]
["6ES78105CC110YA6","SIMATIC S7, STEP7 PROF 2010 SR4 W/O TIA PORTAL, RENTAL LICENSE FOR 50 HOURS, E-SW, SW AND DOCU. ON DVD, LICENSE KEY ON USB STICK , CLASS A, 5 LANGUAGES (GE,EN,FR,IT,SP), EXECUTABLE UNDER WINXPPROF, WINDOWS 7 ULTIMATE, WINDOWS 7 PROFESSIONAL REFERENCE-HW: S7-300/400, C7",569,"TEM",1,"Simatic",0.25700000000000001,0]
["6ES78105CC110YA7","SIMATIC S7 STEP7 PROF 2010 SR4 W/O TIA PORTAL, DATA MEDIUM INCL. TRIAL LICENSE FOR 14 DAYS, E-SW, SW AND DOCU. ON DVD, LICENSE KEY ON DVD, CLASS A, 5 LANGUAGES (GE,EN,FR,IT,SP), EXECUTABLE UNDER WINXPPROF, WINDOWS 7 ULTIMATE, WINDOWS 7 PROFESSIONAL, REFERENCE-HW: S7-300/400, C7",29,"TEM",1,"Simatic",0.215,0]
["6ES78105CC110YC5","SIMATIC S7, STEP7 PROF 2010 SR4 POWERPACK (CHANGEOVER PACKAGE) W/O TIA PORTAL, FROM STEP7 V3.X ... V.5.5 TO STEP7 PROF 2010 SR4, FLOATING LICENSE FOR 1 USER, E-SW, SW AND DOCU. ON DVD, LICENSE KEY ON USB STICK, CLASS A, 5 LANGUAGES (GE,EN,FR,IT,SP), EXECUTABLE UNDER WINXPPROF, WINDOWS 7 ULTIMATE, WINDOWS 7 PROFESSIONAL REFERENCE-HW: S7-300/400, C7",1217,"TEM",1,"Simatic",0.214,0]
["6ES78105CC110YE5","SIMATIC S7, STEP7 PROF 2010 SR4 UPGRADE W/O TIA PORTAL, FLOATING LICENSE FOR 1 USER, E-SW, SW AND DOCU. ON DVD, LICENSE KEY ON USB STICK , CLASS A, 5 LANGUAGES (GE,EN,FR,IT,SP), EXECUTABLE UNDER WINXPPROF, WINDOWS 7 ULTIMATE, WINDOWS 7 PROFESSIONAL REFERENCE-HW: S7-300/400, C7",754,"TEM",1,"Simatic",0.219,0]
["6ES78105CC112YC0","SIMATIC S7, STEP7 PROF 2010 SR3 UNLOCK COPY LICENSE (UCL), UCL POWERPACK (STEP 7 V5.4 TO PROF 2010), FOR 1 INSTALLATION, W/O TIA PORTAL, ONLY VALID COMBINED WITH UNLOCK COPY LICENSE CONTRACT, REQUIRES UCL BASIC PACKAGE MINIMUM ORDER QUANTITY 20 PIECES",730,"TEM",1,"Simatic",0.26500000000000001,0]
["6ES78105CC112YE0","SIMATIC S7, STEP7 PROF 2010 SR4 UNLOCK COPY LICENSE (UCL), UCL UPGRADE (ED 2006 TO 2010) FOR 1 INSTALLATION, W/O TIA PORTAL, ONLY VALID COMBINED WITH UNLOCK COPY LICENSE CONTRACT, REQUIRES UCL BASIC PACKAGE MINIMUM ORDER QUANTITY 20 PIECES",453,"TEM",1,"Simatic",0.26500000000000001,0]
["6ES78105CC122YA0","SIMATIC S7 STEP 7 PROF 2010 SR4/V14, COMBO INCL. TIA PORTAL, UNLOCK COPY LICENSE (UCL), PACKAGE FOR ONE INSTALLATION SOFTWARE AND DOCU ON DVD, MASTER LICENSE KEY ON CD ONLY VALID COMBINED WITH UNLOCK COPY LICENSE CONTRACT",1886,"TEM",1,"Simatic",0.25,0]
["6ES78105CE110YB5","SIMATIC S7 STEP7 Prof 2010 SR4/V14, COMBO INCL. TIA PORTAL, FLOATING LICENSE FOR 1 USER, E-SW, SOFTWARE, DOCU AND LICENSE KEY DOWNLOAD, CLASS A, 5/6 LANGUAGES (G,E,F,I,S)/(CN), EXECUTABLE UNDER WINDOWS XP FOR 2010 ONLY, WINDOWS 7 FOR 2010 & V14, WINDOWS 8.1 FOR V14 ONLY REFERENCE-HW: S7-300/400 (S7-1200/1500) ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY!",3053,"TEM",1,"Simatic",1.4999999999999999E-2,0]
["6ES78105CE110YB6","SIMATIC S7 STEP7 PROF 2010 SR4, RENTAL LICENSE FOR 50 HOURS, W/O TIA PORTAL, E-SW, W/O SW AND DOCU, LICENSE KEY DOWNLOAD, CLASS A, 5 LANGUAGES (G,E,F,I,S), EXECUTABLE UNDER WINXPPROF, WINDOWS 7 ULTIMATE WNDOWS 7 PROFESSIONAL REFERENCE-HW: S7-300/400, C7 ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY!",525,"TEM",1,"Simatic",1.4999999999999999E-2,0]
["6ES78110CA010YX2","SIMATIC S7, S7-GRAPH SOFTWARE UPDATE SERVICE WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE",179,"TEM",1,"Simatic",0.3,0]
["6ES78110CC002YX0","SIMATIC S7, S7-GRAPH EPL-MASTER, ROYALTY-DUTY PER 1 INSTALLATION, ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, E-SW, SW AND DOCU. ON CD, LICENSE KEY ON CD/FD; CLASS A",330,"TEM",1,"Simatic",0.25,0]
["6ES78110CC002YX1","SIMATIC S7, S7-GRAPH EPL-ROYALTY, SINGLE LICENSE F.1 INSTALLATION E-SW, WITHOUT SW AND DOCU., CLASS A, ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",784,"TEM",1,"Simatic",0.05,0]
["6ES78110CC002YX2","SIMATIC S7, S7-GRAPH EPL-MAINTENANCE, MAINTENANCE CHARGE F. ROYALTY FOR 12 MONTHS, ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",179,"TEM",1,"Simatic",0.05,0]
["6ES78110CC060YA5","SIMATIC S7, S7-GRAPH V5.3 FLOATING LICENSE FOR 1 USER E-SW, SW AND DOCU. ON CD, LICENSE KEY ON USB STICK, CLASS A,5 LANGUAGES(G,E,F,I,S), AS OF STEP7 V5.4 SP4 OR SP5 OR STEP7  V5.5 WITH OR W/O SP1, WINXPPROF, WIN 7 PROF/ULTIMATE, REFERENCE-HW: S7-300/400, C7",784,"TEM",1,"Simatic",0.23100000000000001,0]
["6ES78110CC060YE5","SIMATIC S7, S7-GRAPH V5.3 UPGRADE, FLOATING LICENSE FOR 1 USER E-SW, SW AND DOCUMENT. ON CD, LICENSE KEY ON USB STICK, CLASS A,5 LANGUAGES(G,E,F,I,S), AS OF STEP7 V5.4 SP4 OR SP5 OR STEP7  V5.5 WITH OR W/O SP1, WINXPPROF, WIN 7 PROF/ULTIMATE, REFERENCE-HW:S7-300/400, C7",273,"TEM",1,"Simatic",0.26,0]
["6ES78110CC062YN8","SIMATIC S7, S7-GRAPH V5.3 UNLOCK COPY LICENSE, ONLY VALID COMBINED WITH UNLOCK COPY LICENSE CONTRACT AND VALID LICENSE",326,"TEM",1,"Simatic",0.5,0]
["6ES78111CA010YX2","SIMATIC S7, S7-SCL SOFTWARE UPDATE SERVICE WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE",179,"TEM",1,"Simatic",0.3,0]
["6ES78111CC002YX0","SIMATIC S7, S7-SCL EPL-MASTER, ROYALTY-DUTY PER 1 INSTALLATION, ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, E-SW, SW AND DOCU. ON CD, LICENSE KEY ON CD/FD; CLASS A",330,"TEM",1,"Simatic",0.25,0]
["6ES78111CC002YX1","SIMATIC S7, S7-SCL EPL-ROYALTY, SINGLE LICENSE F.1 INSTALLATION E-SW, WITHOUT SW AND DOCU., CLASS A, ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",784,"TEM",1,"Simatic",0.01,0]
["6ES78111CC002YX2","SIMATIC S7, S7-SCL EPL-MAINTENANCE, MAINTENANCE CHARGE F. ROYALTY FOR 12 MONTHS, ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",179,"TEM",1,"Simatic",0.05,0]
["6ES78111CC050YA5","SIMATIC S7, S7-SCL V5.3 FLOATING LICENSE FOR 1 USER E-SW, SW AND DOCU. ON CD, LICENSE KEY ON FD, CLASS A, 5 LANGUAGES (G,E,F,I,S), AS OF STEP 7 V5.4, WINXPPROF, WIN 7 ULTIMATE/PROF, REFERENCE-HW: S7-300/400, C7",784,"TEM",1,"Simatic",0.23300000000000001,0]
["6ES78111CC050YE5","SIMATIC S7, S7-SCL V5.3",273,"TEM",1,"Simatic",0.27200000000000002,0]
["6ES78111CC052YN8","SIMATIC S7, S7-SCL V5.3 UNLOCK COPY LICENSE, ONLY VALID COMBINED WITH UNLOCK COPY LICENSE CONTRACT AND VALID LICENSES ACCORDING TO THE NUMBER OF USERS",326,"TEM",1,"Simatic",0.1,0]
["6ES78200CC002YX0","SIMATIC S7, IMAP, EPL-MASTER, ROYALTY-DUTY PER 1 INSTALLATION, ONLY VALID COMBINED W. ENTERPRISE LICENSE CONTRACT, E-SW, SW AND DOCU. ON CD, LICENSE KEY ON CD/FD; CLASS A",364,"TEM",1,"Simatic",0.25,0]
["6ES78200CC002YX1","SIMATIC S7, IMAP EPL-ROYALTY, SINGLE LICENSE F.1 INSTALLATION E-SW, WITHOUT SW AND DOCU., CLASS A, ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",2202,"TEM",1,"Simatic",0.01,0]
["6ES78200CC002YX2","SIMATIC S7, IMAP EPL-MAINTENANCE, MAINTENANCE CHARGE F. ROYALTY FOR 12 MONTHS, ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",483,"TEM",1,"Simatic",0.01,0]
["6ES78200CC010YX2","SIMATIC S7, IMAP SOFTWARE UPDATE SERVICE WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE",483,"TEM",1,"Simatic",0.1,0]
["6ES78200CC040YA5","SIMATIC S7, IMAP V3.0 FLOATING LICENSE FOR 1 USER, E-SW, SW AND DOCU. ON CD, LICENSE KEY ON USB STICK, CLASS A, 5 LANGUAGES (GE/EN/FR/IT/SP), EXECUTABLE UNDER WINXPPROF, WIN 7 ULTIMATE/PROF, REFERENCE-HW:S7-300/400, ET 200X/S, PROFINET CBA",2202,"TEM",1,"Simatic",0.247,0]
["6ES78200CC040YE5","SIMATIC S7, IMAP V3.0 UPGRADE, FLOATING LICENSE FOR 1 USER, E-SW, SW AND DOCU. ON CD, LICENSE KEY ON USB STICK, CLASS A, 5 LANGUAGES (GE/EN/FR/IT/SP), EXECUTABLE UNDER WINXPPROF, WIN 7 ULTIMATE/PROF, REFERENCE-HW:S7-300/400, ET 200X/S, PROFINET CBA",754,"TEM",1,"Simatic",0.24199999999999999,0]
["6ES78220AA000YL0","SIMATIC S7, STEP 7 BASIC, SOFTWARE UPDATE SERVICE WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE",84,"TEM",1,"Simatic",0.3,0]
["6ES78220AA000YM0","SIMATIC S7, STEP 7 BASIC, SOFTWARE UPDATE SERVICE COMPACT WITH MULTIPLE ORDERS FROM ONE IST SUPPLIES WILL BE COMBINED INTO ONE PACKAGE. MINIMUM QUANTITY ORDER: 3 PCS. WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE. PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE",84,"TEM",1,"Simatic",0.1,0]
["6ES78220AA002YP4","SIMATIC STEP 7 Basic V14 EPL MASTER; ENGINEERING SOFTWARE IN TIA PORTAL; ROYALTY-DUTY PER 1 INSTALLATION; ONLY VALID IN COMBINATION WITH ENTERPRISE LICENSE AGREEMENT; SOFTWARE ON DVD; LICENSE ON CD; CLASS A",309,"TEM",1,"Simatic",0.1,0]
["6ES78220AA030YA5","SIMATIC STEP 7 BASIC V13 SP1 FLOATING LICENSE; ENGINEERING SOFTWARE IN TIA PORTAL; SOFTWARE AND DOCUMENTATION ON DVD; LICENSE KEY ON USB-STICK; CLASS A; 6 LANGUAGES: GE,EN,IT,FR,SP,CN; EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64 BIT), WINDOWS 8.1 (64 BIT); FOR CONFIGURATION OF SIMATIC S7-1200 SIMATIC BASIC PANELS",330,"TEM",1,"Simatic",0.35299999999999998,0]
["6ES78220AA030YA7","SIMATIC STEP 7 BASIC V13 SP1 TRIAL LICENSE FOR 21 DAYS; ENGINEERING SOFTWARE IN TIA PORTAL; SOFTWARE AND DOCUMENTATION ON DVD; CLASS A; 6 LANGUAGES: GE,EN,IT,FR,SP,CN EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64 BIT), WINDOWS 8.1 (64 BIT); FOR CONFIGURATION OF SIMATIC S7-1200 SIMATIC BASIC PANELS",27.700000000000003,"TEM",1,"Simatic",0.34699999999999998,0]
["6ES78220AA030YE5","SIMATIC STEP 7 BASIC V13 SP1 UPGRADE V11..V12 -> V13 FLOATING LICENSE; ENGINEERING SOFTWARE IN TIA PORTAL; SOFTWARE AND DOCUMENTATION ON DVD; LICENSE KEY ON USB-STICK; CLASS A; 6 LANGUAGES: GE,EN,IT,FR,SP,CN; EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64 BIT), WINDOWS 8.1 (64 BIT); FOR CONFIGURATION OF SIMATIC S7-1200 SIMATIC BASIC PANELS",133,"TEM",1,"Simatic",0.35399999999999998,0]
["6ES78220AA040YA5","SIMATIC STEP 7 Basic V14, floating license; engineering software in TIA PORTAL; software and documentation on DVD; license key on USB-STick; class A; 6 languages: GE,EN,IT,FR,SP,CN; executable under Windows 7 (64 BIT), Windows 8.1 (64 BIT); for configuration of SIMATIC S7-1200 SIMATIC Basic Panels",330,"TEM",1,"Simatic",0.39400000000000002,0]
["6ES78220AA040YA7","SIMATIC STEP 7 Basic V14, Trial license for 21 days; engineering software in TIA PORTAL; software and documentation on DVD; class A; 6 languages: GE,EN,IT,FR,SP,CN executable under Windows 7 (64 BIT), Windows 8.1 (64 BIT); for configuration of SIMATIC S7-1200 SIMATIC Basic Panels",27.3,"TEM",1,"Simatic",0.308,0]
["6ES78220AA040YE5","SIMATIC STEP 7 Basic V14, Upgrade V11..V13 -> V14 floating license; engineering software in TIA PORTAL; software and documentation on DVD; license key on USB STick; class A; 6 languages: GE,EN,IT,FR,ES,ZH; executable under Windows 7 (64 BIT), Windows 8.1 (64 BIT); for configuration of SIMATIC S7-1200 SIMATIC Basic Panels",133,"TEM",1,"Simatic",0.39300000000000002,0]
["6ES78220AA044YE5","SIMATIC STEP 7 Basic V14 Trainer Pack Upgrade V14, Engineering-Software; Upgrade for 6x V1x Single/ Floating-> V14 Floating; SW and Documentation on DVD; License-Keys on USB; 6 languages: ge,en,it,fr,sp,cn; executable under Windows 7 (64 Bit); Windows 8.1 (64 Bit); for configuration of SIMATIC S7-1200, SIMATIC Basic Panels; for educational purposes only",175,"TEM",1,"Simatic",0.2,0]
["6ES78220AE000YY0","SIMATIC STEP7 BASIC SUS DOWNLOAD TIA PORTAL WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY",79.5,"TEM",1,"Simatic",1E-3,0]
["6ES78220AE030YA5","SIMATIC STEP 7 BASIC V13 SP1 FLOATING LICENSE DOWNLOAD; ENGINEERING SOFTWARE IN TIA PORTAL; SOFTWARE, DOCUMENTATION AND LICENSE KEY FOR DOWNLOAD; CLASS A; 6 LANGUAGES: GE,EN,IT,FR,SP,CN EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64 BIT), WINDOWS 8.1 (64 BIT); FOR CONFIGURATION OF SIMATIC S7-1200, SIMATIC BASIC PANELS ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY",314,"TEM",1,"Simatic",1E-3,0]
["6ES78220AE030YE5","SIMATIC STEP 7 BASIC V13 SP1 UPGRADE V11..V12 -> V13 FLOATING LICENSE DOWNLOAD; ENGINEERING SOFTWARE IN TIA PORTAL; SOFTWARE, DOCUMENTATION AND LICENSE KEY FOR DOWNLOAD; CLASS A; 6 LANGUAGES: GE,EN,IT,FR,SP,CN EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64 BIT), WINDOWS 8.1 (64 BIT); FOR CONFIGURATION OF SIMATIC S7-1200, SIMATIC BASIC PANELS ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY",126,"TEM",1,"Simatic",1E-3,0]
["6ES78220AE040YA5","SIMATIC STEP 7 Basic V14, floating license download; engineering software in TIA PORTAL; software, documentation and license key for download; class A; 6 languages: GE,EN,IT,FR,SP,CN executable under Windows 7 (64 BIT), Windows 8.1 (64 BIT); for configuration of SIMATIC S7-1200, SIMATIC Basic Panels ******************************* email address is mandatory for delivery",314,"TEM",1,"Simatic",1E-3,0]
["6ES78220AE040YE5","SIMATIC STEP 7 Basic V14, Upgrade V11..V13 -> V14 floating license Download; engineering software in TIA PORTAL; software, documentation and license key for download; class A; 6 languages: GE,EN,IT,FR,ES,ZH; executable under Windows 7 (64 BIT), Windows 8.1 (64 BIT); for configuration of SIMATIC S7-1200, SIMATIC Basic Panels ******************************* email address is mandatory for delivery",126,"TEM",1,"Simatic",1E-3,0]
["6ES78220BE030YE5","SIMATIC STEP 7 BASIC V13 SP1 UPGRADE V10.5 -> V13 FLOATING LICENSE, ENGINEERING SOFTWARE IM TIA PORTAL, SOFTWARE, DOCUMENTATION AND LICENSE KEY FOR DOWNLOAD; CLASS A; 6 LANGUAGES: GE,EN,IT,FR,SP,CN; EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64 BIT), WINDOWS 8.1 (64 BIT); FOR CONFIGURATION OF SIMATIC S7-1200, SIMATIC BASIC PANELS ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY",133,"TEM",1,"Simatic",1E-3,0]
["6ES78220BE040YE5","SIMATIC STEP 7 Basic V14, Upgrade V10.5 -> V14 floating license, engineering software im TIA PORTAL, software, documentation and license key for download; class A; 6 languages: GE,EN,IT,FR,ES,ZH; executable under Windows 7 (64 BIT), Windows 8.1 (64 BIT); for configuration of SIMATIC S7-1200, SIMATIC Basic Panels ******************************* email address is mandatory for delivery",133,"TEM",1,"Simatic",1E-3,0]
["6ES78221AA000YL5","SIMATIC STEP 7 PROFESSIONAL SOFTWARE UPDATE SERVICE (SUS) FOR STEP 7 IM TIA PORTAL; WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE. PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE",420,"TEM",1,"Simatic",0.1,0]
["6ES78221AA000YM5","SIMATIC STEP 7 PROFESSIONAL SOFTWARE UPDATE SERVICE (SUS) COMPACT FOR STEP 7 TIA PORTAL; WITH MULTIPLE ORDERS FROM ONE IST SUPPLIES WILL BE COMBINED INTO ONE PACKAGE. MINIMUM QUANTITY ORDER: 3 PCS. WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE. PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE",420,"TEM",1,"Simatic",0.1,0]
["6ES78221AA002XQ2","SIMATIC STEP 7 Prof. V14 POWERPACK & UPGRADE V5.5 -> V14 COMBO EPL ROYALTY FOR ONE INSTALLATION; WITHOUT SOFTWARE; PRECONDITION IS AN EXISTING STEP 7 V5.X EPL AGREEMENT WITH EPL-MASTER, ROYALTY AND MAINTENANCE; ONLY VALID IN CONJUNCION WITH ORDER OF EPL-MASTER AND EPL-MAINTENANCE 2010/V13; CONTAINS ONLY EPL ROYALTY 2010/V13; CONTAINS NO SOFTWARE AND NO DOCUMENTATION.",368,"TEM",1,"Simatic",0.89500000000000002,0]
["6ES78221AA002YN4","SIMATIC STEP 7 PROFESSIONAL TIA PORTAL EPL MAINTENANCE; MAINTENANCE CHARGE FOR ROYALTY FOR 12 MONTHS; ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT; REQUIRES EPL-MASTER",433,"TEM",1,"Simatic",0.1,0]
["6ES78221AA022YP4","SIMATIC STEP 7 Prof. V14 EPL MASTER; ENGINEERING SOFTWARE IN TIA PORTAL ROYALTY-DUTY PER 1 INSTALLATION; ONLY VALID IN COMBINATION WITH ENTERPRISE LICENSE AGREEMENT; SOFTWARE ON DVD; LICENSE ON CD; CLASS A",309,"TEM",1,"Simatic",0.1,0]
["6ES78221AA022YQ4","SIMATIC STEP 7 Prof. V14 EPL ROYALTY FOR ONE INSTALLATION; WITHOUT SOFTWARE NOR DOCUMENTATION; ONLY VALID COMBINED WITH ENTERPRISE LICENSE AGREEMENT; REQUIRES EPL-MASTER",2086,"TEM",1,"Simatic",0.89500000000000002,0]
["6ES78221AA022YR4","SIMATIC STEP 7 Prof. V14 EPL-ROYALTY FOR SERVICE FOR ONE INSTALLATION; WITHOUT SOFTWARE NOR DOCUMENTATION; ONLY VALID COMBINED WITH ENTERPRISE LICENSE AGREEMENT; REQUIRES EPL-MASTER",2086,"TEM",1,"Simatic",0.89500000000000002,0]
["6ES78221AA030XC2","SIMATIC STEP 7 PROF. V13 SP1 TRANSITION PACKAGE; POWERPACK & UPGRADE STEP 7 V5.4..V5.5 -> V13 COMBO; FLOATING LICENSE; THIS PRODUCT IS ONLY AVAILABLE IN CONJUNCTION WITH ORDER OF SUS 6ES78105CC040YE2. PRECONDITION IS AN EXISTING STEP 7 SUS; SW AND DOCU. ON DVD, CLASS A, LICENSE KEY ON USB STICK , 6 LANGUAGES(GE,EN,IT,FR,SP,CN), EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64BIT), WINDOWS 8.1 (64 BIT); FOR CONFIGURATION OF SIMATIC S7-1200/1500 SIMATIC S7-300/400/WINAC SIMATIC BASIC PANELS",387,"TEM",1,"Simatic",0.215,0]
["6ES78221AA030XC5","SIMATIC STEP 7 PROF. V13 SP1 POWERPACK & UPGRADE STEP 7 V5.4..V5.5 -> V13 COMBO FLOATING LICENSE; ENGINEERING SOFTWARE IN TIA PORTAL; SOFTWARE AND DOCUMENTATION ON DVD; LICENSE KEY ON USB-STICK; CLASS A; 6 LANGUAGES: GE,EN,IT,FR,SP,CN; EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64 BIT), WINDOWS 8.1 (64 BIT); FOR CONFIGURATION OF SIMATIC S7-1200/1500, SIMATIC S7-300/400/WINAC, SIMATIC BASIC PANELS",1379,"TEM",1,"Simatic",0.53200000000000003,0]
["6ES78221AA030XE5","SIMATIC STEP 7 PROF. V13 SP1 UPGRADE 2006..2010 -> V13 COMBO FLOATING LICENSE; ENGINEERING SOFTWARE IN TIA PORTAL; SOFTWARE AND DOCUMENTATION ON DVD; LICENSE KEY ON USB-STICK; CLASS A; 6 LANGUAGES: GE,EN,IT,FR,SP,CN; EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64 BIT), WINDOWS 8.1 (64 BIT); FOR CONFIGURATION OF SIMATIC S7-1200/1500, SIMATIC S7-300/400/WINAC, SIMATIC BASIC PANELS",834,"TEM",1,"Simatic",0.52800000000000002,0]
["6ES78221AA030YA5","SIMATIC STEP 7 PROF. V13 SP1 FLOATING LICENSE; ENGINEERING SOFTWARE IN TIA PORTAL; SOFTWARE AND DOCUMENTATION ON DVD; LICENSE KEY ON USB-STICK; CLASS A; 6 LANGUAGES: GE,EN,IT,FR,SP,CN; EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64 BIT), WINDOWS 8.1 (64 BIT); FOR CONFIGURATION OF SIMATIC S7-1200/1500, SIMATIC S7-300/400/WINAC, SIMATIC BASIC PANELS",2086,"TEM",1,"Simatic",0.46400000000000002,0]
["6ES78221AA030YA7","SIMATIC STEP 7 PROF. V13 SP1 TRIAL FOR 21 DAYS; ENGINEERING SOFTWARE IN TIA PORTAL; SOFTWARE AND DOCUMENTATION ON DVD; CLASS A; 6 LANGUAGES: GE,EN,IT,FR,SP,CN; EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64 BIT), WINDOWS 8.1 (64 BIT); FOR CONFIGURATION OF SIMATIC S7-1200/1500, SIMATIC S7-300/400/WINAC, SIMATIC BASIC PANELS",27.700000000000003,"TEM",1,"Simatic",0.438,0]
["6ES78221AA030YC5","SIMATIC STEP 7 PROF. V13 SP1 POWERPACK BASIC V13 -> PROFESSIONAL V13 FLOATING LICENSE; ENGINEERING SOFTWARE IN TIA PORTAL; SOFTWARE AND DOCUMENTATION ON DVD; LICENSE KEY ON USB-STICK; CLASS A; 6 LANGUAGES: GE,EN,IT,FR,SP,CN; EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64 BIT), WINDOWS 8.1 (64 BIT); FOR CONFIGURATION OF SIMATIC S7-1200/1500, SIMATIC S7-300/400/WINAC, SIMATIC BASIC PANELS",1766,"TEM",1,"Simatic",0.442,0]
["6ES78221AA030YE5","SIMATIC STEP 7 PROF. V13 SP1 UPGRADE V11..V12 -> V13 OR V11..V12 COMBO -> V13 COMBO FLOATING LICENSE; ENGINEERING SOFTWARE IN TIA PORTAL; ALSO VALID FOR UPGRADING V11 SINGLE LICENSES; SOFTWARE AND DOCUMENTATION ON DVD; LICENSE KEY ON USB-STICK; CLASS A; 6 LANGUAGES: GE,EN,IT,FR,SP,CN; EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64 BIT), WINDOWS 8.1 (64 BIT); FOR CONFIGURATION OF SIMATIC S7-1200/1500, SIMATIC S7-300/400/WINAC, SIMATIC BASIC PANELS",834,"TEM",1,"Simatic",0.52400000000000002,0]
["6ES78221AA032XC6","SIMATIC STEP 7 PROF. V13 SP1 POWERPACK & UPGRADE V5.X -> V13 COMBO UCL (2010 AND TIA PORTAL) FOR ONE INSTALLATION; ENGINEERING-SOFTWARE; SOFTWARE AND DOCUMENTATION ON DVD; MASTER LICENSE ON CD; ONLY VALID WITH UCL AGREEMENT",828,"TEM",1,"Simatic",0.89500000000000002,0]
["6ES78221AA032XE6","SIMATIC STEP 7 PROF. V13 SP1 UPGRADE 2006..2010 -> V13 COMBO UCL (2010 AND TIA PORTAL) FOR ONE INSTALLATION ENGINEERING-SOFTWARE; SOFTWARE AND DOCUMENTATION ON DVD; MASTER LICENSE ON CD; ONLY VALID WITH UCL AGREEMENT",668,"TEM",1,"Simatic",0.2,0]
["6ES78221AA032YA6","SIMATIC STEP 7 PROF. V13 SP1 UCL PACKAGE (TIA PORTAL) FOR ONE INSTALLATION; ENGINEERING-SOFTWARE; SOFTWARE AND DOCUMENTATION ON DVD; MASTER LICENSE ON CD; ONLY VALID WITH UCL AGREEMENT",1668,"TEM",1,"Simatic",0.89500000000000002,0]
["6ES78221AA032YE6","SIMATIC STEP 7 PROF. V13 SP1 UPGRADE V11..V12 -> V13 UCL (TIA PORTAL) FOR ONE INSTALLATION ENGINEERING-SOFTWARE; SOFTWARE AND DOCUMENTATION ON DVD; MASTER LICENSE ON CD; ONLY VALID WITH UCL AGREEMENT",667,"TEM",1,"Simatic",0.89500000000000002,0]
["6ES78221AA034YE5","SIMATIC STEP 7 PROFESSIONAL 2010 SR4 / V13 SP1 COMBO TRAINER PACK UPGRADE; STEP 7 PROFESSIONAL V13 SP1, STEP 7 PROFESIONAL 2010 SR4, DISTRIBUTED SAFETY V5.4, S7-TECHNOLOGY V4.2, FLOATING LICENSE FOR 12 USER; SOFTWARE AND DOCUMENTATION ON DVD; LICENSE KEY ON USB-STICK; CLASS A; 6 LANGUAGES: GE,EN,IT,FR,SP,CN; EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64 BIT); FOR CONFIGURATION OF SIMATIC S7-1500/1200/300/400/WINAC, SIMATIC BASIC PANELS, 3 X SW. FOR 20 STUDENTS V13 (6ES7822-1AC03-4YA5), FOR EDUCATIONAL PURPOSES ONLY",1307,"TEM",1,"Simatic",8.76,0]
["6ES78221AA040XC2","SIMATIC STEP 7 Prof. V14, Transition Package; Powerpack & Upgrade STEP 7 V5.4..V5.5 -> V14 Combo; floating license; this product is only available in conjunction with order of SUS 6ES78105CC040YE2. precondition is an exiSTing STEP 7 SUS; SW and Docu. On DVD, class A, license key on USB STick , 6 languages(GE,EN,IT,FR,ES,ZH), executable under Windows 7 (64BIT), Windows 8.1 (64 BIT); for configuration of SIMATIC S7-1200/1500 SIMATIC S7-300/400/WinAC SIMATIC Basic Panels",387,"TEM",1,"Simatic",0.215,0]
["6ES78221AA040XC5","SIMATIC STEP 7 Prof. V14, Powerpack & Upgrade STEP 7 V5.4..V5.5 -> V14 Combo floating license; engineering software in TIA PORTAL; software and documentation on DVD; license key on USB STick; class A; 6 languages: GE,EN,IT,FR,ES,ZH; executable under Windows 7 (64 BIT), Windows 8.1 (64 BIT); for configuration of SIMATIC S7-1200/1500, SIMATIC S7-300/400/WinAC, SIMATIC Basic Panels",1379,"TEM",1,"Simatic",0.59199999999999997,0]
["6ES78221AA040XE5","SIMATIC STEP 7 Prof. V14, Upgrade 2006..2010 -> V14 Combo floating license; engineering software in TIA PORTAL; software and documentation on DVD; license key on USB STick; class A; 6 languages: GE,EN,IT,FR,ES,ZH; executable under Windows 7 (64 BIT), Windows 8.1 (64 BIT); for configuration of SIMATIC S7-1200/1500, SIMATIC S7-300/400/WinAC, SIMATIC Basic Panels",834,"TEM",1,"Simatic",0.59099999999999997,0]
["6ES78221AA040YA5","SIMATIC STEP 7 Prof. V14, floating license; engineering software in TIA PORTAL; software and documentation on DVD; license key on USB STick; class A; 6 languages: GE,EN,IT,FR,ES,ZH; executable under Windows 7 (64 BIT), Windows 8.1 (64 BIT); for configuration of SIMATIC S7-1200/1500, SIMATIC S7-300/400/WinAC, SIMATIC Basic Panels",2086,"TEM",1,"Simatic",0.52,0]
["6ES78221AA040YA7","SIMATIC STEP 7 Prof. V14, trial for 21 days; engineering software in TIA PORTAL; software and documentation on DVD; class A; 6 languages: GE,EN,IT,FR,ES,ZH; executable under Windows 7 (64 BIT), Windows 8.1 (64 BIT); for configuration of SIMATIC S7-1200/1500, SIMATIC S7-300/400/WinAC, SIMATIC Basic Panels",27.700000000000003,"TEM",1,"Simatic",0.40100000000000002,0]
["6ES78221AA040YC5","SIMATIC STEP 7 Prof. V14, Powerpack Basic V14 -> Professional V14 floating license; engineering software in TIA PORTAL; software and documentation on DVD; license key on USB STick; class A; 6 languages: GE,EN,IT,FR,ES,ZH; executable under Windows 7 (64 BIT), Windows 8.1 (64 BIT); for configuration of SIMATIC S7-1200/1500, SIMATIC S7-300/400/WinAC, SIMATIC Basic Panels",1766,"TEM",1,"Simatic",0.504,0]
["6ES78221AA040YE5","SIMATIC STEP 7 Prof. V14, Upgrade V11..V13 -> V14 or V11..V13 Combo -> V14 Combo floating license; engineering software in TIA PORTAL; also valid for upgrading V11 single licenses; software and documentation on DVD; license key on USB STick; class A; 6 languages: GE,EN,IT,FR,ES,ZH; executable under Windows 7 (64 BIT), Windows 8.1 (64 BIT); for configuration of SIMATIC S7-1200/1500, SIMATIC S7-300/400/WinAC, SIMATIC Basic Panels",834,"TEM",1,"Simatic",0.501,0]
["6ES78221AA042XC6","SIMATIC STEP 7 Prof. V14, Powerpack & Upgrade V5.X -> V14 Combo UCL (2010 and TIA PORTAL) for one inSTallation; engineering software; Software and Documentation on DVD; MaSTer License on CD; only valid with UCL agreement",828,"TEM",1,"Simatic",0.89500000000000002,0]
["6ES78221AA042XE6","SIMATIC STEP 7 Prof. V14, Upgrade 2006..2010 -> V14 Combo UCL (2010 and TIA PORTAL) for one inSTallation engineering software; software and documentation on DVD; MaSTer License on CD; only valid with UCL agreement",668,"TEM",1,"Simatic",0.89500000000000002,0]
["6ES78221AA042YA6","SIMATIC STEP 7 Prof. V14, UCL Package (TIA PORTAL) for one inSTallation; engineering software; software and documentation on DVD; MaSTer License on CD; only valid with UCL agreement",1668,"TEM",1,"Simatic",0.89500000000000002,0]
["6ES78221AA042YE6","SIMATIC STEP 7 Prof. V14, Upgrade V11..V12 -> V14 UCL (TIA PORTAL) for one inSTallation engineering software; Software and Documentation on DVD; MaSTer License on CD; only valid with UCL agreement",667,"TEM",1,"Simatic",0.89500000000000002,0]
["6ES78221AA044YA5","SIMATIC STEP 7 Professional 2010 SR4/V14 Combo Software for Training; STEP7 Professional Combo, Safety Combo, S7-PLCSIM Advanced, OPC UA, Cloud Connector Floating-License for 1 User; SW and Docu on DVD, Class A, 6 languages: ge,en,it,fr,sp,cn; executable under Windows 7 (64 BIT); for configuration of SIMATIC S7-1200/1500, SIMATIC S7-300/400/WINAC, SIMATIC Basic Panels; for educational purposes only",485,"TEM",1,"Simatic",1.2,0]
["6ES78221AA044YE5","SIMATIC STEP7 Professional 2010 SR4/V14 Combo Trainer Pack; STEP7 Professional Combo, Safety Combo, S7-PLCSIM Advanced, OPC UA, Cloud Connector Floating-License for 6 user; SW and Docu on DVD, Class A, license key on USB-STick; 6 languages: ge,en,it,fr,sp,cn; executable under Windows 7 (64 BIT); for configuration of SIMATIC S7-1500/1200/300/400/WinAC, SIMATIC Basic Panels; 1x SW for 20 STudents V14 (6ES7822-1AC04-4YA5), for educational purposes only",485,"TEM",1,"Simatic",1.2,0]
["6ES78221AC044YA5","SIMATIC STEP 7 Professional V14/2010 SR4 Combo, Safety Combo Engineering-Software for 20 STudents; 20 Trial licenses for 365 days on USB-STick, software and documentation on DVD; 6 languages: ge,en,it,fr,sp,cn; executable under Windows 7 (64 Bit); for configuration of SIMATIC S7-1200/1500, SIMATIC S7-300/400/WINAC, SIMATIC Basic Panels for educational purposes only",245,"TEM",1,"Simatic",0.3,0]
["6ES78221AD044YA5","SIMATIC STEP 7 Professional V14/2010 SR4 Combo, Safety Combo Engineering-Software for 100 STudents; 100 Trial licenses for 365 days on USB-STick, software and documentation on DVD; 6 languages: ge,en,it,fr,sp,cn; executable under Windows 7 (64 Bit); for configuration of SIMATIC S7-1200/1500, SIMATIC S7-300/400/WINAC, SIMATIC Basic Panels for educational purposes only",138,"TEM",1,"Simatic",0.3,0]
["6ES78221AE000YY0","SIMATIC STEP 7 PROFESSIONAL SOFTWARE UPDATE SERVICE (SUS) DOWNLOAD FOR TIA PORTAL; WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE. PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY",399,"TEM",1,"Simatic",1E-3,0]
["6ES78221AE030XC2","SIMATIC STEP 7 PROF. V13 SP1 TRANSITION PACKAGE DOWNLOAD; POWERPACK & UPGRADE STEP 7 V5.5 -> V13 COMBO FLOATING LICENSE; THIS PRODUCT IS ONLY AVAILABLE IN CONJUNCTION WITH ORDER OF SUS 6ES7810-5CC04-0YY2 PRECONDITION IS AN EXISTING STEP 7 SUS; CLASS A; SOFTWARE,DOCUMENTATION AND LICENSE KEY AS DOWNLOAD; 6 LANGUAGES(GE,EN,IT,FR,SP,CN), EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64BIT), WINDOWS 8.1 (64 BIT); ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY",368,"TEM",1,"Simatic",1E-3,0]
["6ES78221AE030XC5","SIMATIC STEP 7 PROF. V13 SP1 POWERPACK & UPGRADE STEP 7 V5.4..V5.5 -> V13 COMBO FLOATING LICENSE DOWNLOAD; ENGINEERING SOFTWARE IN TIA PORTAL; SOFTWARE, DOCUMENTATION AND LICENSE KEY FOR DOWNLOAD; CLASS A; 6 LANGUAGES: GE,EN,IT,FR,SP,CN; EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64BIT), WINDOWS 8.1 (64 BIT); FOR CONFIGURATION OF SIMATIC S7-1200/1500, SIMATIC S7-300/400/WINAC, SIMATIC BASIC PANELS ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY",1313,"TEM",1,"Simatic",1E-3,0]
["6ES78221AE030XE5","SIMATIC STEP 7 PROF. V13 SP1 UPGRADE 2006..2010 -> V13 COMBO FLOATING LICENSE DOWNLOAD; ENGINEERING SOFTWARE IN TIA PORTAL; SOFTWARE, DOCUMENTATION AND LICENSE KEY FOR DOWNLOAD; CLASS A; 6 LANGUAGES: GE,EN,IT,FR,SP,CN; EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64BIT), WINDOWS 8.1 (64 BIT); FOR CONFIGURATION OF SIMATIC S7-1200/1500, SIMATIC S7-300/400/WINAC, SIMATIC BASIC PANELS ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY",794,"TEM",1,"Simatic",1E-3,0]
["6ES78221AE030YA5","SIMATIC STEP 7 PROF. V13 SP1 FLOATING LICENSE DOWNLOAD; ENGINEERING SOFTWARE IN TIA PORTAL; SOFTWARE, DOCUMENTATION AND LICENSE KEY FOR DOWNLOAD; CLASS A; 6 LANGUAGES: GE,EN,IT,FR,SP,CN; EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64BIT), WINDOWS 8.1 (64 BIT); FOR CONFIGURATION OF SIMATIC S7-1200/1500, SIMATIC S7-300/400/WINAC, SIMATIC BASIC PANELS ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY",1985,"TEM",1,"Simatic",1E-3,0]
["6ES78221AE030YC5","SIMATIC STEP 7 PROF. V13 SP1 POWERPACK BASIC V13 -> PROFESSIONAL V13 FLOATING LICENSE DOWNLOAD; ENGINEERING SOFTWARE IN TIA PORTAL; SOFTWARE, DOCUMENTATION AND LICENSE KEY FOR DOWNLOAD; CLASS A; 6 LANGUAGES: GE,EN,IT,FR,SP,CN; EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64BIT), WINDOWS 8.1 (64 BIT); FOR CONFIGURATION OF SIMATIC S7-1200/1500, SIMATIC S7-300/400/WINAC, SIMATIC BASIC PANELS ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY",1680,"TEM",1,"Simatic",1E-3,0]
["6ES78221AE030YE5","SIMATIC STEP 7 PROF. V13 SP1 UPGRADE V11..V12 -> V13 OR V11..V12 COMBO -> V13 COMBO FLOATING LICENSE DOWNLOAD; ENGINEERING SOFTWARE IN TIA PORTAL; ALSO VALID FOR UPGRADING V11 SINGLE LICENSES; SOFTWARE, DOCUMENTATION AND LICENSE KEY FOR DOWNLOAD; CLASS A; 6 LANGUAGES: GE,EN,IT,FR,SP,CN; EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64BIT), WINDOWS 8.1 (64 BIT); ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY",794,"TEM",1,"Simatic",1E-3,0]
["6ES78221AE040XC2","SIMATIC STEP 7 Prof. V14, Transition Package Download; Powerpack & Upgrade STEP 7 V5.5 -> V14 Combo floating license; this product is only available in conjunction with order of SUS 6ES7810-5CC04-0YY2 precondition is an exiSTing STEP 7 SUS; class A; Software,Documentation and license key AS Download; 6 languages(GE,EN,IT,FR,ES,ZH), executable under Windows 7 (64BIT), Windows 8.1 (64 BIT); ******************************* email address is mandatory for delivery",368,"TEM",1,"Simatic",1E-3,0]
["6ES78221AE040XC5","SIMATIC STEP 7 Prof. V14, Powerpack & Upgrade STEP 7 V5.4..V5.5 -> V14 Combo floating license download; engineering software in TIA PORTAL; software, documentation and license key for Download; class A; 6 languages: GE,EN,IT,FR,ES,ZH; executable under Windows 7 (64BIT), Windows 8.1 (64 BIT); for configuration of SIMATIC S7-1200/1500, SIMATIC S7-300/400/WinAC, SIMATIC Basic Panels ******************************* email address is mandatory for delivery",1313,"TEM",1,"Simatic",1E-3,0]
["6ES78221AE040XE5","SIMATIC STEP 7 Prof. V14, Upgrade 2006..2010 -> V14 Combo floating license download; engineering software in TIA PORTAL; software, documentation and license key for download; class A; 6 languages: GE,EN,IT,FR,ES,ZH; executable under Windows 7 (64BIT), Windows 8.1 (64 BIT); for configuration of SIMATIC S7-1200/1500, SIMATIC S7-300/400/WinAC, SIMATIC Basic Panels ******************************* email address is mandatory for delivery",794,"TEM",1,"Simatic",1E-3,0]
["6ES78221AE040YA5","SIMATIC STEP 7 Prof. V14, floating license download; engineering software in TIA PORTAL; software, documentation and license key for download; class A; 6 languages: GE,EN,IT,FR,ES,ZH; executable under Windows 7 (64BIT), Windows 8.1 (64 BIT); for configuration of SIMATIC S7-1200/1500, SIMATIC S7-300/400/WinAC, SIMATIC Basic Panels ******************************* email address is mandatory for delivery",1985,"TEM",1,"Simatic",1E-3,0]
["6ES78221AE040YC5","SIMATIC STEP 7 Prof. V14, Powerpack Basic V14 -> Professional V14 floating license download; engineering software in TIA PORTAL; software, documentation and license key for download; class A; 6 languages: GE,EN,IT,FR,ES,ZH; executable under Windows 7 (64BIT), Windows 8.1 (64 BIT); for configuration of SIMATIC S7-1200/1500, SIMATIC S7-300/400/WinAC, SIMATIC Basic Panels ******************************* email address is mandatory for delivery",1680,"TEM",1,"Simatic",1E-3,0]
["6ES78221AE040YE5","SIMATIC STEP 7 Prof. V14, Upgrade V11..V13 -> V14 or V11..V13 Combo -> V14 Combo floating license download; engineering software in TIA PORTAL; also valid for upgrading V11 single licenses; software, documentation and license key for download; class A; 6 languages: GE,EN,IT,FR,ES,ZH; executable under Windows 7 (64BIT), Windows 8.1 (64 BIT); ******************************* email address is mandatory for delivery",794,"TEM",1,"Simatic",1E-3,0]
["6ES78221BA030XE5","SIMATIC STEP 7 PROF. V13 SP1 UPGRADE V13 -> V13 COMBO FLOATING LICENSE; ENGINEERING SOFTWARE IN TIA PORTAL; SOFTWARE AND DOCUMENTATION ON DVD; LICENSE KEY ON USB-STICK; CLASS A; 6 LANGUAGES: GE,EN,IT,FR,SP,CN; EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64 BIT), WINDOWS 8.1 (64 BIT); FOR CONFIGURATION OF SIMATIC S7-1200/1500, SIMATIC S7-300/400/WINAC, SIMATIC BASIC PANELS",1082,"TEM",1,"Simatic",0.23,0]
["6ES78221BA034YA5","SIMATIC STEP 7 PROFESSIONAL 2010 SR4 / V13 SP1 COMBO TRAINER PACK; STEP 7 PROFESSIONAL V13 SP1, STEP 7 PROFESSIONAL 2010 SR4, DISTRIBUTED SAFETY V5.4, S7-TECHNOLOGY V4.2, FLOATING LICENSE FOR 12 USER; SOFTWARE AND DOCUMENTATION ON DVD; LICENSE KEY ON USB-STICK; CLASS A; 6 LANGUAGES: GE,EN,IT,FR,SP,CN; EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64 BIT); FOR CONFIGURATION OF SIMATIC S7-1500/1200/300/400/WINAC, SIMATIC BASIC PANELS; 3 X SW FOR 20 STUDENTS V13 SP1 (6ES7822-1AC03-4YA5), FOR EDUCATIONAL PURPOSES ONLY",3919,"TEM",1,"Simatic",8.77,0]
["6ES78221BA034YE5","SIMATIC STEP 7 PROFESSIONAL 2010 SR4 / V13 SP1 COMBO COMPANY UPGRADE, STEP 7 PROFESSIONAL V13 SP1, STEP 7 PROFESSIONAL 2010 SR4, DISTRIBUTED SAFETY V5.4, S7-TECHNOLOGY V4.2, FLOATING LICENSE FOR 12 USER; SW AND DOCU ON DVD, CLASS A, 6 LANGUAGES: GE,EN,IT,FR,SP,CN; EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64 BIT); FOR CONFIGURATION OF SIMATIC S7-1500/1200/300/400/WINAC, SIMATIC BASIC PANELS, FOR EDUCATIONAL PURPOSES ONLY",1307,"TEM",1,"Simatic",1.2,0]
["6ES78221BA040XE5","SIMATIC STEP 7 Prof. V14, Upgrade V14-> V14/2010 Combo Floating License; Engineering Software in TIA PORTAL; Software and Documentation on DVD; License key ON USB-STick; class A; 6 languages: GE,EN,IT,FR,ES,ZH; executable under Windows 7 (64 BIT), Windows 8.1 (64 BIT); for configuration of SIMATIC S7-1200/1500, SIMATIC S7-300/400/WinAC, SIMATIC Basic Panels",1082,"TEM",1,"Simatic",0.504,0]
["6ES78221BA044YA5","SIMATIC STEP7 Professional 2010 SR4/V14 Combo Trainer Pack; STEP7 Professional Combo, Safety Combo, S7-PLCSIM Advanced, OPC UA, Cloud Connector Floating-License for 6 user; SW and Docu on DVD, Class A, license key on USB-STick; 6 languages: ge,en,it,fr,sp,cn; executable under Windows 7 (64 BIT); for configuration of SIMATIC S7-1500/1200/300/400/WinAC, SIMATIC Basic Panels; 1x SW for 20 STudents V14 (6ES7822-1AC04-4YA5), for educational purposes only",1628,"TEM",1,"Simatic",1.2,0]
["6ES78221BE030YC5","SIMATIC STEP 7 PROF. V13 SP1 POWERPACK V13 TRIAL 365 -> V13 FLOATING LICENSE DOWNLOAD; ENGINEERING SOFTWARE IN TIA PORTAL; THIS PRODUCT IS ONLY AVAILABLE IN CONJUNCTION WITH ORDER OF SUS 6ES78221AE000YY0; PRECONDITION IS AN EXISTING STEP 7 V13 SP1 TRIAL 365 LICENSE; LICENSE KEY FOR DOWNLOAD W/O SW AND W/O DOCU. ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY",834,"TEM",1,"Simatic",1E-3,0]
["6ES78221BE040YC5","SIMATIC STEP 7 Prof. V14, Powerpack V14 Trial 365 -> V14 Floating License Download; Engineering Software in TIA PORTAL; this product is only available in conjunction with order of SUS 6ES78221AE000YY0; precondition is an exiSTing STEP 7 V14 Trial 365 License; License key for Download w/o SW and w/o Docu. ******************************* email address is mandatory for delivery",834,"TEM",1,"Simatic",1E-3,0]
["6ES78221XA002YQ4","SIMATIC STEP 7 Prof. V14 EPL-ROYALTY; ROYALTY FOR 1 INSTALLATION; ONLY VALID COMBINED WITH ENTERPRISE LICENSE AGREEMENT; 00011-GB8; REQUIRES EPL-MASTER",1985,"TEM",1,"Simatic",0.89500000000000002,0]
["6ES78221XA002YR4","SIMATIC STEP 7 Prof. V14 EPL ROYALTY FOR SERVICE; ROYALTY FOR 1 INSTALLATION; ONLY VALID COMBINED WITH ENTERPRISE LICENSE AGREEMENT; 00011-GB8; REQUIRES EPL-MASTER",1985,"TEM",1,"Simatic",0.89500000000000002,0]
["6ES78230AA001AA0","SIMATIC ProDiag S7-1500, Single Runtime License, contains certificate of license for 250 supervisions, class A, running on all S7-1500 from firmware V2.0",174,"TEM",1,"Simatic",1.2E-2,0]
["6ES78230AE001AA0","SIMATIC ProDiag S7-1500, Single Runtime License Download contains certificate of license for 250 supervisions, as pdf for download, class A, running on all S7-1500 from firmware V2.0 ******************************* email address is mandatory for delivery",158,"TEM",1,"Simatic",1E-3,0]
["6ES78230BA001BA0","SIMATIC OPC UA S7-1500 Small, single runtime license, contains certificate of license OPC UA Server (Data Access), class A, running on every ET 200SP CPU, S7-1500 up to CPU-1513, 1505S incl. F and T derivates from firmware V2.0",116,"TEM",1,"Simatic",1.6E-2,0]
["6ES78230BA001CA0","SIMATIC OPC UA S7-1500 Medium, single runtime license, contains certificate of license OPC UA Server (Data Access), class A, running on every ET 200SP CPU, S7-1500 up to CPU-1516, 1505S and 1507S incl. F and T derivates from firmware V2.0",231,"TEM",1,"Simatic",1.4999999999999999E-2,0]
["6ES78230BA001DA0","SIMATIC OPC UA S7-1500 Large, single runtime license, contains certificate of license OPC UA Server (Data Access), class A, running on every ET 200SP CPU, every S7-1500 CPU, 1505S and 1507S incl. F and T derivates from firmware V2.0",347,"TEM",1,"Simatic",1.4E-2,0]
["6ES78230BE001BA0","SIMATIC OPC UA S7-1500 Small, single runtime license download contains certificate of license OPC UA Server (Data Access), class A, running on every ET 200SP CPU, S7-1500 up to CPU-1513, 1505S incl. F and T derivates from firmware V2.0 ******************************* e-mail address is mandatory for delivery",105,"TEM",1,"Simatic",1E-3,0]
["6ES78230BE001CA0","SIMATIC OPC UA S7-1500 Medium, single runtime license download contains certificate of license OPC UA Server (Data Access), class A, running on every ET 200SP CPU, S7-1500 up to CPU-1516, 1505S and 1507S incl. F and T derivates from firmware V2.0 ******************************* e-mail address is mandatory for delivery",210,"TEM",1,"Simatic",1E-3,0]
["6ES78230BE001DA0","SIMATIC OPC UA S7-1500 Large, single runtime license download contains certificate of license OPC UA Server (Data Access), class A, running on every ET 200SP CPU, every S7-1500 CPU, 1505S and 1507S incl. F and T derivates from firmware V2.0 ******************************* e-mail address is mandatory for delivery",315,"TEM",1,"Simatic",1E-3,0]
["6ES78231AA000YL5","TIA Portal Multiuser Engineering Software Update Service (SUS); Within the framwork of this contract, you will receive updated software versions for a period of one year. Extended by another year, if it is not canceled three months prior to its expiration. Period of delivery and performance: 1 year from date of invoice prerequisite for contract: current version of the software",116,"TEM",1,"Simatic",0.3,0]
["6ES78231AA002YN4","TIA Portal Multiuser Engineering TIA Portal EPL Maintenance; maintenance charge for royalty for 12 months; only valid combined with Enterprise License Contract; requires EPL-MaSTer",116,"TEM",1,"Simatic",0.89500000000000002,0]
["6ES78231AA002YP4","TIA Portal Multiuser Engineering V14 EPL MaSTer option for engineering software in TIA Portal Royalty-Duty per 1 InSTallation; only valid in combination with Enterprise License Agreement; Software on STEP7 / WinCC DVD; license on CD; class A",231,"TEM",1,"Simatic",0.1,0]
["6ES78231AA002YQ4","TIA Portal Multiuser Engineering V14 EPL Royalty for one inSTallation; without software nor documentation; only valid in combination with Enterprise License Agreement; requires EPL-MaSTer",578,"TEM",1,"Simatic",0.89500000000000002,0]
["6ES78231AA040YA5","TIA Portal Multiuser Engineering V14 floating license download; option for engineering software in TIA Portal; software and documentation on STEP 7 / WinCC DVD license key on USB STick; class A; 6 languages: ge,en,it,fr,sp,cn; executable under Windows 7 (64Bit), Windows 8.1 (64 Bit);",578,"TEM",1,"Simatic",0.14899999999999999,0]
["6ES78231AA042YA6","TIA Portal Multiuser Engineering V14 UCL package for one inSTallation; Engineering-Software; software and documentation on STEP 7 / WinCC DVD; maSTer license on CD; only valid with UCL agreement",462,"TEM",1,"Simatic",0.2,0]
["6ES78231AA042YL6","TIA Portal Multiuser Engineering Software Update Service for UCL Unlock Copy License, automatic supply of upgrades and service packs for one year with automatic renewal, requires lateST software version, only valid combined with Unlock Copy License contract",92.4,"TEM",1,"Simatic",0.1,0]
["6ES78231AE000YL5","TIA Portal Multiuser Engineering SUS (Download) Software Update Service; Within the framwork of this contract, you will receive updated software versions for a period of one year. Extended by another year, if it is not canceled three months prior to its expiration. Period of delivery and performance: 1 year from date of invoice prerequisite for contract: current version of the software ******************************* email address is mandatory for delivery",105,"TEM",1,"Simatic",1E-3,0]
["6ES78231AE002YN4","TIA Portal Multiuser Engineering EPL Maintenance download; maintenance charge for royalty for 12 months; only valid combined with Enterprise License Contract; requires EPL-MaSTer ******************************* email address is mandatory for delivery",105,"TEM",1,"Simatic",1E-3,0]
["6ES78231AE002YP4","TIA Portal Multiuser Engineering V14 EPL MaSTer download option for engineering software in TIA Portal Royalty-Duty per 1 InSTallation; only valid in combination with Enterprise License Agreement; Software with STEP 7 / WinCC download; license for download; class A ******************************* email address is mandatory for delivery",210,"TEM",1,"Simatic",1E-3,0]
["6ES78231AE002YQ4","TIA Portal Multiuser Engineering V14 EPL Royalty download for one inSTallation; without software nor documentation; only valid in combination with Enterprise License Agreement; requires EPL-MaSTer ******************************* email address is mandatory for delivery",525,"TEM",1,"Simatic",1E-3,0]
["6ES78231AE040YA5","TIA Portal Multiuser Engineering V14 floating License download; option for engineering software in TIA Portal; software and docu contained in STEP 7 / WinCC download; license key for download; class A; 6 languages: DE,EN,IT,FR,ES,ZH; executable under Windows 7 (64Bit), Windows 8.1 (64 Bit); ******************************* email address is mandatory for delivery",525,"TEM",1,"Simatic",1E-3,0]
["6ES78231AE042YA6","TIA Portal Multiuser Engineering V14 UCL package (download) for one inSTallation; Engineering-Software; software and docu contained in STEP 7 / WinCC download; maSTer license for download; only valid with UCL agreement ******************************* email address is mandatory for delivery",420,"TEM",1,"Simatic",1E-3,0]
["6ES78231AE042YL6","TIA Portal Multiuser Engineering Software Update Service for UCL Unlock Copy License, download, automatic supply of upgrades and service packs for one year with automatic renewal, requires lateST software version only valid combined with Unlock Copy License contract ******************************* email address is mandatory for delivery",84,"TEM",1,"Simatic",1E-3,0]
["6ES78231BE000YA5","SIMATIC Target 1500S (TM) for Simulink(R) V1.0 Single License Download; Engineering Software Software, Documentation and License cert. for download; Class A; 2 languages: Ge,En; Executable under Windows 7 (64 Bit); Windows 8.1 (64 Bit) Software for integration of Simulink models to the S7 program of S7-1500 SW Controller and CPU 1518 ODK; ******************************* E-mail address is mandatory for delivery",1575,"TEM",1,"Simatic",1E-3,0]
["6ES78231BE100YA0","Target 1500S + ODK 1500S Bundle Contains: SIMATIC ODK 1500S V2.0 and SIMATIC Target 1500S (TM) for Simulink (R) V1.0, Single License Download, E-SW, SW Documentation and License certific. for download, Class A, 2 languages: ge,en, Executable under Windows 7 (64 Bit), Windows 8.1 (64 Bit), Software for integration of Simulink models to the S7-program of S7-1500 SW Controller and CPU 1518 ODK ******************************* E-mail address is mandatory for delivery",3150,"TEM",1,"Simatic",1E-3,0]
["6ES78231CA000YA0","TIA Portal Cloud Connector single license; for use with separately licensed TIA Portal products, which are released for the Cloud Connec tor, according to \"Specific Terms for the Use of Software in Connection with the TIA Portal Cloud Connector\" https://siemens.com/ cloud-connector-info; software and documentation on STEP7/WinCC DVD; license key on USB-STick; class A; 6 languages: ge,en,it,fr,sp,cn; executable under Win 7(64 Bit), Win 8.1(64 Bit), Win 10(64 Bit)",405,"TEM",1,"Simatic",0.15,0]
["6ES78231CE000YA0","TIA Portal Cloud Connector single license download; for use with separately licensed TIA Portal products, which are released for the Cloud Connec tor, according to \"Specific Terms for the Use of Software in Connection with the TIA Portal Cloud Connector\" https://siemens.com/ cloud-connector-info; sw and docu with STEP 7/WinCC download; license key for download; class A; 6 languages: ge,en,it,fr,sp,cn; executable under Win 7(64 Bit), Win 8.1(64 Bit), Win 10(64 Bit) ******************************* e-mail address is mandatory for delivery",368,"TEM",1,"Simatic",1E-3,0]
["6ES78231EA000YA5","TIA Portal Teamcenter Gateway floating license contains certificate of license Tia Portal Teamcenter Gateway V14 SW und documentaion on DVD; license key on USB STick class A;",1155,"TEM",1,"Simatic",0.2,0]
["6ES78231EA000YL5","TIA Portal Teamcenter Gateway software update service (SUS) for TIA Portal Teamcenter Gateway; Under this contract you will receive updated software versions for a period of one year. This will be extended for another year if not cancelled three months prior to its expiration date. Period of delivery and performance: 1 year from the date of invoice Prerequisite for contract: Current version of the software",231,"TEM",1,"Simatic",0.3,0]
["6ES78231EE000YA5","TIA Portal Teamcenter Gateway download - floating license contains certificate of license Tia Portal Teamcenter Gateway V14 class A; compatibility only between TIA Portal V14 and Teamcenter V11.2 ******************************* email address is mandatory for delivery",1050,"TEM",1,"Simatic",1E-3,0]
["6ES78231EE000YL5","TIA Portal Teamcenter Gateway software update service (SUS) for TIA Portal Teamcenter Gateway download version; Under this contract you will receive updated software versions for a period of one year. This will be extended for another year if not cancelled three months prior to its expiration date. Period of delivery and performance: 1 year from the date of invoice Prerequisite for contract: Current version of the software ******************************* email address is mandatory for delivery",210,"TEM",1,"Simatic",1E-3,0]
["6ES78231FA000YA5","SIMATIC S7-PLCSIM Advanced V1.0 floating license; option for simulation of S7-1500 & ET200SP; SW and documentation on DVD, license key on USB STick; class A; SW 1 language: en, Docu 2 languages: ge,en; executable under Windows 7 (64 bit),",2888,"TEM",1,"Simatic",0.223,0]
["6ES78231FA000YL5","SIMATIC S7-PLCSIM Advanced Software Update Service (SUS); Within the framwork of this contract, you will receive updated software versions for a period of one year. Extended by another year, if it is not canceled three months prior to its expiration. Period of delivery and performance: 1 year from date of invoice prerequisite for contract: current version of the software",578,"TEM",1,"Simatic",0.3,0]
["6ES78231FA002YN4","SIMATIC S7-PLCSIM Advanced V1.0 TIA Portal EPL Maintenance; maintenance charge for royalty for 12 months; only valid combined with Enterprise License Contract; requires EPL-MaSTer",578,"TEM",1,"Simatic",0.89500000000000002,0]
["6ES78231FA002YP4","SIMATIC S7-PLCSIM Advanced V1.0 EPL MaSTer option for simulation of S7-1500 & ET200SP; Royalty-Duty per 1 InSTallation; only valid in combination with Enterprise License Agreement; Software on DVD; license on CD; class A",1155,"TEM",1,"Simatic",0.2,0]
["6ES78231FA002YQ4","SIMATIC S7-PLCSIM Advanced V1.0 EPL Royalty for one inSTallation; without software nor documentation; only valid in combination with Enterprise License Agreement; requires EPL-MaSTer",2888,"TEM",1,"Simatic",0.89500000000000002,0]
["6ES78231FE000YA5","SIMATIC S7-PLCSIM Advanced V1.0 floating License download; option for simulation of S7-1500 & ET200SP; software, documentation and license key for download; class A; SW 1 language: en, Docu 2 languages: ge,en; executable under Windows 7 (64Bit), ******************************* email address is mandatory for delivery",2625,"TEM",1,"Simatic",1E-3,0]
["6ES78231FE000YL5","SIMATIC S7-PLCSIM Advanced SUS (Download) Software Update Service; Within the framwork of this contract, you will receive updated software versions for a period of one year. Extended by another year, if it is not canceled three months prior to its expiration. Period of delivery and performance: 1 year from date of invoice prerequisite for contract: current version of the software ******************************* email address is mandatory for delivery",525,"TEM",1,"Simatic",1E-3,0]
["6ES78231FE002YN4","SIMATIC S7-PLCSIM Advanced V1.0 EPL Maintenance download; maintenance charge for royalty for 12 months; only valid combined with Enterprise License Contract; requires EPL-MaSTer ******************************* email address is mandatory for delivery",525,"TEM",1,"Simatic",1E-3,0]
["6ES78231FE002YP4","SIMATIC S7-PLCSIM Advanced V1.0 EPL MaSTer download option for simulation of S7-1500 & ET200SP; Royalty-Duty per 1 InSTallation; only valid in combination with Enterprise License Agreement; Software and licenskey for download; class A ******************************* email address is mandatory for delivery",1050,"TEM",1,"Simatic",1E-3,0]
["6ES78231FE002YQ4","SIMATIC S7-PLCSIM Advanced V1.0 EPL Royalty download for one inSTallation; without software nor documentation; only valid in combination with Enterprise License Agreement; requires EPL-MaSTer ******************************* email address is mandatory for delivery",2625,"TEM",1,"Simatic",1E-3,0]
["6ES78231GE040YA5","SIMATIC 50h Eng. V14 Combo floating license download; 50h actual use of the following SIMATIC Engineering Software: STEP 7 Professional 2010 SR4, STEP 7 Professional V14, WinCC flexible 2008, WinCC Professional V14, STEP 7 DiSTributed Safety V5.4, STEP 7 Safety Advanced V14; software, documentation and license key for download; class A; ******************************* e-mail address is mandatory for delivery",515,"TEM",1,"Simatic",1E-3,0]
["6ES78301AA102YE0","SIMATIC S7, MODULAR PID CONTROL V5.1 SP1, PARAMETR.SW AND FB, EPL-MASTER, ROYALTY-DUTY PER 1 INSTALLATION, E-SW AND R-SW, SW AND DOCU. ON CD, LICENSE KEY ON CD; CLASS A, 2 LANGUAGES (G,E), EXECUT. F. STEP7 V5.3 SP2 ONLY VALID COMBINED WITH ENTERPRISE LICENSE-CONTRACT",332,"TEM",1,"Simatic",1.0069999999999999,0]
["6ES78301AA102YE1","SIMATIC S7, MODULAR PID CONTROL V5.1, PARAMETR.SW, EPL-ROYALTY, SINGLE LICENSE F.1 INSTALLATION E-SW, WITHOUT SW AND DOCU., CLASS A, 2 LANGUAGES (G,E), EXECUT. F. STEP7 V5.3 SP2 ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",399,"TEM",1,"Simatic",0.01,0]
["6ES78301AA102YE2","SIMATIC S7, MODULAR PID CONTROL V5.1, PARAMETR.SW, EPL-MAINTENANCE, MAINTENANCE CHARGE F. ROYALITY FOR 12 MONTHS, ONLY VALID COMBINED WITH ENTERPRISE LICENSE-CONTRACT, REQUIRES EPL-MASTER",99.800000000000011,"TEM",1,"Simatic",0.01,0]
["6ES78301AA110YX0","SIMATIC S7, MODULAR PID CONTROL V5.1, PARAMETR.SW, FLOATING LICENSE FOR 1 INSTALLATION E-SW, SW AND DOCU ON CD, LICENSE KEY ON USB-STICK, CLASS A, 2 LANGUAGES (G,E), EXECUTABLE UNDER STEP7 AB V5.3 SP2",399,"TEM",1,"Simatic",0.22600000000000001,0]
["6ES78302AA220YX0","SIMATIC S7, STANDARD PID CONTROL V5.2, PARAMETR.SW, FLOATING LICENSE FOR 1 INSTALLATION, E-SW, SW AND DOCU. ON CD, LICENSE KEY ON USB-STICK, CLASS A, 2 LANGUAGES (G,E), EXECUTABLE UNDER STEP7 FROM V5.3 SP2",424,"TEM",1,"Simatic",0.21,0]
["6ES78331FA002YX0","SIMATIC S7, F PROGRAMMING TOOL, STEP 7 SAFETY ADVANCED; EPL-MASTER, ROYALTY-DUTY PER 1 INSTALLATION, ONLY VALID COMBINED WITH ENTERPRISE LICENCE CONTRACT E-SW, SW AND DOCU. ON DVD LICENSE KEY ON CD/FD, LANGUAGES (G,E), EXECUTABLE UNDER TIA PORTAL V14 FROM STEP 7 PROFESSIONAL V14",309,"TEM",1,"Simatic",0.2,0]
["6ES78331FA130YA5","SIMATIC S7, F PROGRAMMING TOOL, STEP 7 SAFETY ADVANCED V13 SP1; ENGINEERING-SW; FLOATING LICENSE FOR 1 USER; SOFTWARE AND DOCU. ON DVD; LICENSE KEY ON USB-STICK; CLASS A, 2 LANGUAGES (G,E); EXECUTABLE UNDER TIA PORTAL V13 SP1 FROM STEP7 PROFESSIONAL V13 SP1",616,"TEM",1,"Simatic",0.26400000000000001,0]
["6ES78331FA130YA8","SIMATIC S7, F PROGRAMMING TOOL STEP 7 SAFETY ADVANCED V13 SP1 TRIAL FOR 21 DAYS; ENGINEERING-SW; SOFTWARE AND DOCU. ON DVD; CLASS A, 2 LANGUAGES (G,E); EXECUTABLE UNDER TIA PORTAL V13 SP1 FROM STEP 7 PROF. V13 SP1; FOR CONFIGURATION OF SIMATIC S7-1200F/1500F, SIMATIC S7-300F/400F/WINAC F",27.700000000000003,"TEM",1,"Simatic",0.23799999999999999,0]
["6ES78331FA130YC5","SIMATIC S7, F PROGRAMMING TOOL STEP 7 SAFETY ADVANCED POWERPACK BASIC V13 SP1 -> ADVANCED V13 SP1; ENGINEERING-SW; FLOATING LICENSE FOR 1 USER; LICENSE KEY ON USB-STICK; CLASS A, 2 LANGUAGES (G,E); EXECUTABLE UNDER TIA PORTAL V13 SP1 FROM STEP 7 PROF. V13 SP1; FOR CONFIGURATION OF SIMATIC S7-1200F/1500F, SIMATIC S7-300F/400F/WINAC F",523,"TEM",1,"Simatic",0.158,0]
["6ES78331FA130YE5","SIMATIC S7, F PROGRAMMING TOOL, STEP 7 SAFETY ADVANCED V13 SP1; UPGRADE V11..V12 -> V13 OR V11..V12 COMBO -> V13 COMBO; FOR PARALLEL USING OF STEP 7 SAFETY ADVANCED V11/V12 AND STEP 7 SAFETY ADVANCED V13; ENGINEERING-SW; UPGRADE LICENSE; SOFTWARE AND DOCU. ON DVD; LICENSE KEY ON USB-STICK; CLASS A, 2 LANGUAGES (G,E); EXECUTABLE UNDER TIA PORTAL V13 SP1 FROM STEP7 PROFESSIONAL V13 SP1",247,"TEM",1,"Simatic",0.251,0]
["6ES78331FA130YF5","SIMATIC S7, F PROGRAMMING TOOL, STEP 7 SAFETY ADVANCED V13 SP1; UPGRADE DISTRIBUTED SAFETY V5.4 SP5 -> V13 COMBO; FOR PARALLEL USING OF DISTRIBUTED SAFETY V5.4 SP5, AND STEP 7 SAFETY ADVANCED V13; ENGINEERING-SW; UPGRADE COMBO LICENSE SOFTWARE AND DOCU. ON DVD; LICENSE KEY ON USB-STICK; CLASS A, 2 LANGUAGES (G,E); EXECUTABLE UNDER TIA PORTAL V13 SP1 FROM STEP7 PROFESSIONAL V13 SP1",247,"TEM",1,"Simatic",0.25600000000000001,0]
["6ES78331FA130YH5","SIMATIC S7, F PROGRAMMING TOOL, STEP 7 SAFETY ADVANCED V13 SP1; ENGINEERING-SW; FLOATING LICENSE FOR 1 USER, SOFTWARE, DOCUMENTATION AND LICENSE KEY FOR DOWNLOAD; CLASS A, 2 LANGUAGES (GE,EN); EXECUTABLE UNDER TIA PORTAL V13 SP1 FROM STEP7 PROFESSIONAL V13 SP1 ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY",588,"TEM",1,"Simatic",1E-3,0]
["6ES78331FA130YJ5","SIMATIC S7, F PROGRAMMING TOOL STEP 7 SAFETY ADVANCED POWERPACK BASIC V13 SP1 -> ADVANCED V13 SP1; ENGINEERING-SW; FLOATING LICENSE FOR 1 USER; LICENSE KEY FOR DOWNLOAD; CLASS A, 2 LANGUAGES (GE,EN); EXECUTABLE UNDER TIA PORTAL V13 SP1 FROM STEP 7 PROF. V13 SP1; FOR CONFIGURATION OF SIMATIC S7-1200F/1500F, SIMATIC S7-300F/400F/WINAC F; ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY",497,"TEM",1,"Simatic",1E-3,0]
["6ES78331FA130YK5","SIMATIC S7, F PROGRAMMING TOOL, STEP 7 SAFETY ADVANCED V13 SP1; UPGRADE V11..V12 -> V13 OR V11..V12 COMBO -> V13 COMBO; FOR PARALLEL USING OF STEP 7 SAFETY ADVANCED V11/V12 AND STEP 7 SAFETY ADVANCED V13; ENGINEERING-SW; UPGRADE LICENSE; SOFTWARE, DOCUMENTATION AND LICENSE KEY FOR DOWNLOAD; CLASS A, 2 LANGUAGES (GE,EN); EXECUTABLE UNDER TIA PORTAL V13 SP1 FROM STEP7 PROFESSIONAL V13 SP1 ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY",236,"TEM",1,"Simatic",1E-3,0]
["6ES78331FA130YY5","SIMATIC S7, F PROGRAMMING TOOL, STEP 7 SAFETY ADVANCED V13 SP1; UPGRADE DISTRIBUTED SAFETY V5.4 SP5 -> V13 COMBO; FOR PARALLEL USING OF DISTRIBUTED SAFETY V5.4 SP5, AND STEP 7 SAFETY ADVANCED V13; ENGINEERING-SW; UPGRADE COMBO LICENSE SOFTWARE, DOCUMENTATION AND LICENSE KEY FOR DOWNLOAD; CLASS A, 2 LANGUAGES (GE,EN); EXECUTABLE UNDER TIA PORTAL V13 SP1 FROM STEP7 PROFESSIONAL V13 SP1 ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY",236,"TEM",1,"Simatic",1E-3,0]
["6ES78331FA132YA0","SIMATIC S7, F PROGRAMMING TOOL, STEP 7 SAFETY ADVANCED V13 SP1; UNLOCK COPY LICENSE (UCL); PACKAGE FOR ONE INSTALLATION; ENGINEERING-SOFTWARE; SOFTWARE AND DOKU ON DVD; MASTER LICENSE KEY ON CD; LANGUAGES (G,E), CLASS A; EXECUTABLE UNDER TIA PORTAL V13 SP1 FROM STEP7 PROFESSIONAL V13 SP1 ONLY VALID COMBINED WITH UCL CONTRACT",352,"TEM",1,"Simatic",0.2,0]
["6ES78331FA132YE0","SIMATIC S7, F PROGRAMMING TOOL, STEP 7 SAFETY ADVANCED V13 SP1; UNLOCK COPY LICENSE (UCL); UPGRADE DSITRIBUTED SAFETY V5.4 -> STEP 7 SAFETY ADVANCED V13; PACKAGE FOR ONE INSTALLATION; ENGINEERING-SOFTWARE; SOFTWARE AND DOCU ON DVD; MASTER LICENSE KEY ON CD; 2 LANGUAGES (G,E), CLASS A; EXECUTABLE UNDER TIA PORTAL V13 SP1 FROM STEP7 PROFESSIONAL V13 SP1 ONLY VALID COMBINED WITH UCL CONTRACT",141,"TEM",1,"Simatic",0.2,0]
["6ES78331FA132YQ0","SIMATIC S7, F PROGRAMMING TOOL, STEP 7 SAFETY ADVANCED V14; EPL-ROYALTY; SINGLE LICENSE FOR ONE INSTALLATION; ESW, W/O SW AND DOCU.; ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT; REQUIRES EPL-MASTER",616,"TEM",1,"Simatic",0.2,0]
["6ES78331FA132YQ1","SIMATIC S7, F PROGRAMMING TOOL, STEP 7 SAFETY ADVANCED V14; EPL-ROYALTY SERVICE; SINGLE LICENSE FOR ONE INSTALLATION; E-SW, W/O SW AND DOCU.; KLASSE A; ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT; REQUIRES EPL-MASTER",616,"TEM",1,"Simatic",0.2,0]
["6ES78331FA132YR0","SIMATIC S7, F PROGRAMMING TOOL, STEP 7 SAFETY ADVANCED V14; EPL-MAINTENANCE; MAINTENANCE CHARGE F. ROYALTY; FOR 12 MONTHS; ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT; REQUIRES EPL-MASTER",147,"TEM",1,"Simatic",0.2,0]
["6ES78331FA132YS0","SIMATIC S7, F-Programming-Tool, STEP 7 Safety Advanced V14; EPL-Royalty Upgrade DiSTributed Safety V5.4 -> V14 Combo; Single License f.1 inSTallation E-SW, without SW and Docu.; Class A; only valid combined with Enterprise License Contract; requires EPL-MaSTer",247,"TEM",1,"Simatic",0.2,0]
["6ES78331FA140YA5","SIMATIC S7, F-Programming Tool, STEP 7 Safety Advanced V14; Engineering-Software; Floating License for 1 User; Software and Docu. on DVD; License Key on USB-STick; Class A, 2 Languages (ge,en); executable under TIA Portal V14 from STEP 7 Professional V14; for configuration of SIMATIC S7-1200F/1500F, SIMATIC S7-1500F SW Controller, SIMATIC S7-300F/400F/WINAC F",616,"TEM",1,"Simatic",0.33500000000000002,0]
["6ES78331FA140YA8","SIMATIC S7, F Programming Tool STEP 7 Safety Advanced V14 Trial for 21 days; Engineering-Software; Software and Docu. on DVD; Class A, 2 Languages (ge,en); executable under TIA Portal V14 from STEP 7 Professional V14; for configuration of SIMATIC S7-1200F/1500F, SIMATIC S7-1500F SW Controller, SIMATIC S7-300F/400F/WINAC F;",27.700000000000003,"TEM",1,"Simatic",0.32800000000000001,0]
["6ES78331FA140YC5","SIMATIC S7, F Programming Tool STEP 7 Safety Advanced Powerpack Basic V14 -> Advanced V14; Engineering-Software; Floating License for 1 User; License Key on USB-STick; Class A, 2 Languages (ge,en); executable under TIA Portal V14 from STEP 7 Professional V14; for configuration of SIMATIC S7-1200F/1500F, SIMATIC S7-1500F SW Controller, SIMATIC S7-300F/400F/WINAC F;",523,"TEM",1,"Simatic",0.2,0]
["6ES78331FA140YE5","SIMATIC S7, F Programming Tool STEP 7 Safety Advanced V14, Upgrade V11..V13-> V14 or V11..V13 combo-> V14 combo; for parallel using of STEP 7 Safety Advanced V11..V13 and STEP 7 Safety Advanced V14; Engineering-SW; Upgrade License for 1 User; Software and Docu. on DVD; License Key on USB-STick; Class A, 2 Languages (ge,en); executable under TIA Portal V14 from STEP 7 Professional V14; for configuration of SIMATIC S7-1200F/1500F, SIMATIC S7-1500F SW Controller, SIMATIC S7-300F/400F/WINAC F;",247,"TEM",1,"Simatic",0.33800000000000002,0]
["6ES78331FA140YF5","SIMATIC S7, F Programming Tool, STEP 7 Safety Advanced V14, Upgrade DiSTributed Safety V5.4 SP5-> V14 Combo; for parallel using of DiSTributed Safety V5.4 SP5, and STEP 7 Safety Advanced V14; Engineering-SW; Upgrade Combo License; Software and Docu. on DVD; License Key on USB-STick; Class A, 2 Languages (ge,en); executable under TIA Portal V14 from STEP 7 Professional V14; for configuration of SIMATIC S7-1200F/1500F, SIMATIC S7-1500F SW Controller, SIMATIC S7-300F/400F/WINAC F;",247,"TEM",1,"Simatic",0.33700000000000002,0]
["6ES78331FA140YH5","SIMATIC S7, F Programming Tool, STEP 7 Safety Advanced V14; Engineering-Software; Floating License for 1 User; Software, Documentation and License Key for Download; Class A, 2 Languages (ge,en); executable under TIA Portal V14 from STEP 7 Professional V14; for configuration of SIMATIC S7-1200F/1500F, SIMATIC S7-1500F SW Controller, SIMATIC S7-300F/400F/WINAC F; ******************************* E-mail address is mandatory for delivery;",588,"TEM",1,"Simatic",1E-3,0]
["6ES78331FA140YJ5","SIMATIC S7, F Programming Tool, STEP 7 Safety Advanced Powerpack Basic V14 -> Advanced V14; Engineering-Software; Floating License for 1 User; License Key for Download; Class A, 2 Languages (ge,en); executable under TIA Portal V14 from STEP 7 Professional V14; for configuration of SIMATIC S7-1200F/1500F, SIMATIC S7-1500F SW Controller, SIMATIC S7-300F/400F/WINAC F; ******************************* E-mail address is mandatory for delivery;",497,"TEM",1,"Simatic",1E-3,0]
["6ES78331FA140YK5","SIMATIC S7, F Programming Tool, STEP 7 Safety Advanced V14, Upgrade V11..V13 -> V14 or V11..V14 Combo -> V14 Combo; for parallel using of STEP 7 Safety Advanced V11..V13 and STEP 7 Safety Advanced V14; Engineering-Software; Upgrade License; Software, Documentation and License Key for Download; Class A, 2 Languages (ge,en); executable under TIA Portal V14 from STEP 7 Professional V14; ******************************* E-mail address is mandatory for delivery;",236,"TEM",1,"Simatic",1E-3,0]
["6ES78331FA140YY5","SIMATIC S7, F Programming Tool, STEP 7 Safety Advanced V14, Upgrade DiSTributed Safety V5.4 SP5-> V14 Combo; for parallel using of DiSTributed Safety V5.4 SP5, and STEP 7 Safety Advanced V14; Engineering-SW; Upgrade Combo License; Software, Documentation and License Key for Download; Class A, 2 Languages (ge,en); executable under TIA Portal V14 from STEP 7 Professional V14; ******************************* E-mail address is mandatory for delivery;",236,"TEM",1,"Simatic",1E-3,0]
["6ES78331FA142YA0","SIMATIC S7, F Programming Tool STEP 7 Safety Advanced V14; Unlock Copy License (UCL); Package for one InSTallation; Engineering-SW; Software and Docu. on DVD; MaSTer License Key on CD; Class A, 2 Languages (ge,en); executable under TIA Portal V14 from STEP 7 Professional V14; for configuration of SIMATIC S7-1200F/1500F, SIMATIC S7-1500F SW Controller, SIMATIC S7-300F/400F/WINAC F; ONLY VALID COMBINED WITH UCL CONTRACT",352,"TEM",1,"Simatic",0.2,0]
["6ES78331FA142YE0","SIMATIC S7, F Programming Tool, STEP 7 Safety Advanced V14, Unlock Copy License (UCL); Upgrade DiSTributed Safety V5.4 -> STEP 7 Safety Advanced V14; Package for one inSTallation; Engineering-Software; Software and Docu. on DVD; MaSTer License Key on CD; Class A, 2 Languages (ge,en); executable under TIA Portal V14 from STEP 7 Professional V14; for configuration of SIMATIC S7-1200F/1500F, SIMATIC S7-1500F SW Controller, SIMATIC S7-300F/400F/WINAC F; only valid combined with UCL contract",141,"TEM",1,"Simatic",0.2,0]
["6ES78331FB130YA5","SIMATIC S7, F PROGRAMMING TOOL STEP 7 SAFETY BASIC V13 SP1; ENGINEERING-SW; FLOATING LICENSE FOR 1 USER; SOFTWARE AND DOCU. ON DVD; LICENSE KEY ON USB-STICK; CLASS A, 2 LANGUAGES (G,E); EXECUTABLE UNDER  TIA PORTAL V13 SP1 FROM STEP 7 BASIC V13 SP1; FOR CONFIGURATION OF SIMATIC S7-1200F",188,"TEM",1,"Simatic",0.25600000000000001,0]
["6ES78331FB130YH5","SIMATIC S7, F PROGRAMMING TOOL STEP 7 SAFETY BASIC V13 SP1; ENGINEERING-SW; FLOATING LICENSE FOR 1 USER; SOFTWARE, DOCUMENTATION AND LICENSE KEY FOR DOWNLOAD; CLASS A, 2 LANGUAGES (GE,EN); EXECUTABLE UNDER  TIA PORTAL V13 SP1 FROM STEP 7 BASIC V13 SP1; FOR CONFIGURATION OF SIMATIC S7-1200F; ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY",179,"TEM",1,"Simatic",1E-3,0]
["6ES78331FB140YA5","SIMATIC S7, F Programming Tool STEP 7 Safety Basic V14; Engineering-Software; Floating License for 1 User; Software and Docu. on DVD; License Key on USB-STick; Class A, 2 Languages (ge,en); executable under TIA Portal V14 from STEP 7 Basic V14; for configuration of SIMATIC S7-1200F",188,"TEM",1,"Simatic",0.33500000000000002,0]
["6ES78331FB140YE5","SIMATIC S7, F Programming Tool, STEP 7 Safety Basic V14, Upgrade V13 SP1 -> V14; for parallel using of STEP 7 Safety Basic V13 SP1 and STEP 7 Safety Basic V14; Engineering-Software; Upgrade License for 1 User; Software and Docu. on DVD; License Key on USB-STick; Class A, 2 Languages (ge,en); executable under TIA Portal V14 from STEP 7 Basic V14; for configuration of SIMATIC S7-1200F",75.600000000000009,"TEM",1,"Simatic",0.33400000000000002,0]
["6ES78331FB140YH5","SIMATIC S7, F Programming Tool, STEP 7 Safety Basic V14; Engineering-Software; Floating License for 1 User; Software, Documentation and License Key for Download; Class A, 2 Languages (ge,en); executable under TIA Portal V14 from STEP 7 Basic V14; for configuration of SIMATIC S7-1200F ******************************* E-mail address is mandatory for delivery;",179,"TEM",1,"Simatic",1E-3,0]
["6ES78331FB140YK5","SIMATIC S7, F Programming Tool, STEP 7 Safety Basic V14, Upgrade V13 SP1 -> V14; for parallel using of STEP 7 Safety Basic V13 SP1 and STEP 7 Safety Basic V14; Engineering-Software; Upgrade License for 1 User; Software, Documentation and License Key for Download; Class A, 2 Languages (ge,en); executable under TIA Portal V14 from STEP 7 Basic V14; for configuration of SIMATIC S7-1200F ******************************* E-mail address is mandatory for delivery;",71.400000000000006,"TEM",1,"Simatic",1E-3,0]
["6ES78331FC000YL0","STEP 7 SAFETY ADVANCED F PROGRAMMING TOOL SUS FOR UCL UNLOCK COPY LICENSE, SOFTWARE UPDATE SERVICE WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE PREREQUISITE FOR CONTRACT: UNLOCK COPY LICENSE CONTRACT",92.4,"TEM",1,"Simatic",0.1,0]
["6ES78331FC000YM2","SIMATIC S7, F PROGRAMMING TOOL STEP 7 SAFETY ADVANCED, SOFTWARE UPDATE SERVICE COMPACT WITH MULTIPLE ORDERS FROM ONE IST SUPPLIES WILL BE COMBINED INTO ONE PACKAGE. MINIMUM QUANTITY ORDER: 3 PCS. WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE. PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE",129,"TEM",1,"Simatic",0.1,0]
["6ES78331FC000YX2","SIMATIC S7, F PROGRAMMING TOOL, STEP 7 SAFETY ADVANCED, SOFTWARE UPDATE SERVICE WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE",131,"TEM",1,"Simatic",0.1,0]
["6ES78331FC000YY0","SIMATIC S7, F PROGRAMMING TOOL STEP 7 SAFETY ADVANCED, SOFTWARE UPDATE SERVICE DOWNLD WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE. PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY",124,"TEM",1,"Simatic",1E-3,0]
["6ES78331FC002YX0","SIMATIC S7, F-Programming-Tool, STEP 7 Safety Advanced Combo V14 / DiSTributed Safety V5.4 EPL-MaSTer, Royalty-Duty per 1 inSTallation; E-SW, SW and Docu. on DVD; License Key on CD/FD; Languages (G, E), Class A; ONLY VALID COMBINED WITH ENTERPRISE LICENCE CONTRACT",345,"TEM",1,"Simatic",0.5,0]
["6ES78331FC002YX1","SIMATIC S7, F-Programming-Tool, STEP 7 Safety Advanced Combo V14 / DiSTributed Safety V5.4 EPL-Royalty, single license f.1 inSTallation E-SW, without SW and Docu.; Class A; only valid combined with Enterprise License Contract; requires EPL-MaSTer",779,"TEM",1,"Simatic",0.05,0]
["6ES78331FC002YX2","SIMATIC S7, F-Programming-Tool, STEP 7 Safety Advanced Combo V14 / DiSTributed Safety V5.4 EPL-Maintenance; Maintenance Charge f. Royalty for 12 month; only valid combined with Enterprise License Contract; requires EPL-MaSTer",154,"TEM",1,"Simatic",1E-3,0]
["6ES78331FC020YA5","SIMATIC S7, F PROGRAMMING TOOL S7 DISTRIBUTED SAFETY V5.4, FLOATING LICENSE FOR 1 USER, E-SW, SW AND DOCU. ON CD, CLASS A, 3 LANGUAGES (G,E,F), EXECUTABLE UNDER STEP7 V5.3 SP3",627,"TEM",1,"Simatic",0.24099999999999999,0]
["6ES78331FC020YE5","SIMATIC S7, F PROGRAMMING TOOL S7 DISTRIBUTED SAFETY V5.4, UPGRADE FROM V5.X TO V5.4, FLOATING LICENSE FOR 1 USER, E-SW, SW AND DOCU. ON CD, CLASS A, 3 LANGUAGES (G,E,F), EXECUTABLE UNDER STEP7 V5.3 SP3",242,"TEM",1,"Simatic",0.24099999999999999,0]
["6ES78331FC020YH5","SIMATIC S7, F PROGRAMMING TOOL S7 DISTRIBUTED SAFETY V5.4, LICENSE KEY DOWNLOAD FLOATING LICENSE FOR 1 USER, E-SW, W/O SW AND DOCU, CLASS A, 3 LANGUAGES (G,E,F), EXECUTABLE UNDER STEP7 V5.3 SP3 ******************************* E-MAIL ADDRESS MANDATORY FOR DELIVERY",569,"TEM",1,"Simatic",1.4999999999999999E-2,0]
["6ES78331FC022YA0","SIMATIC S7, DISTRIBUTED SAFETY UNLOCK COPY LICENSE (UCL), PACKAGE FOR ONE INSTALLATION, ENGINEERING-SOFTWARE SOFTWARE AND DOCUMENTATION ON DVD MASTER LICENSE KEY ON CD ONLY VALID WITH UCL AGREEMENT",377,"TEM",1,"Simatic",0.25700000000000001,0]
["6ES78331FD000YM2","SIMATIC S7, F PROGRAMMING TOOL, STEP 7 SAFETY BASIC, SOFTWARE UPDATE SERVICE COMPACT WITH MULTIPLE ORDERS FROM ONE IST SUPPLIES WILL BE COMBINED INTO ONE PACKAGE. MINIMUM QUANTITY ORDER: 3 PCS. WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE. PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE",51.5,"TEM",1,"Simatic",0.1,0]
["6ES78331FD000YN2","SIMATIC S7, F PROGRAMMING TOOL, STEP 7 SAFETY BASIC, SOFTWARE UPDATE SERVICE DOWNLD WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE. PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY",49.400000000000006,"TEM",1,"Simatic",1E-3,0]
["6ES78331FD000YX2","SIMATIC S7, F PROGRAMMING TOOL, STEP 7 SAFETY BASIC, SOFTWARE UPDATE SERVICE WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE",51.5,"TEM",1,"Simatic",0.1,0]
["6ES78331XF002YQ4","SIMATIC S7, SAFETY ADVANCED V14 EPL-ROYALTY; ROYALTY FOR 1 INSTALLATION; ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT: 00011-GB8; REQUIRES EPL-MASTER",577,"TEM",1,"Simatic",0.2,0]
["6ES78331XF002YR4","SIMATIC S7, SAFETY ADVANCED V14 EPL-ROYALTY FOR SERVICE; ROYALTY FOR 1 INSTALLATION; ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT: 00011-GB8; REQUIRES EPL-MASTER",577,"TEM",1,"Simatic",0.2,0]
["6ES78400CA010YX2","SIMATIC S7, S7-PDIAG SOFTWARE UPDATE SERVICE WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE",242,"TEM",1,"Simatic",0.3,0]
["6ES78400CC002YX0","SIMATIC S7, S7-PDIAG EPL-MASTER, ROYALTY-DUTY PER 1 INSTALLATION, ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT E-SW, SW AND DOCU. ON CD LICENSE KEY ON CD/FD; CLASS A",485,"TEM",1,"Simatic",0.25,0]
["6ES78400CC002YX1","SIMATIC S7, S7-PDIAG EPL-ROYALTY, SINGLE LICENSE F.1 INSTALLATION E-SW, WITHOUT SW AND DOCU., CLASS A, ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",1525,"TEM",1,"Simatic",0.05,0]
["6ES78400CC002YX2","SIMATIC S7, S7-PDIAG EPL-MAINTENANCE, MAINTENANCE CHARGE F. ROYALTY FOR 12 MONTHS, ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",317,"TEM",1,"Simatic",0.1,0]
["6ES78400CC040YA5","SIMATIC S7, S7-PDIAG V5.3 FLOATING LICENSE FOR 1 USER E-SW, SW AND DOCU. ON CD, LICENSE KEY ON USB STICK, CLASS A, 5 LANGUAGES (GE, EN, FR, IT, SP), EXECUTABLE FROM STEP7 V5.4, WINXPPROF, WINDOWS 7 ULTIMATE, WINDOWS 7 PROFESSIONAL, REFERENCE-HW:SIMATIC S7-300/400",1525,"TEM",1,"Simatic",0.22700000000000001,0]
["6ES78400CC040YE5","SIMATIC S7, S7-PDIAG V5.3 UPGRADE, FLOATING LICENSE FOR 1 USER E-SW, SW AND DOCUMENTAT. ON CD, LICENSE KEY ON USB STICK, CLASS A, 5 LANGUAGES (GE, EN, FR, IT, SP), EXECUTABLE FROM STEP7 V5.4, WINXPPROF, WINDOWS 7 ULTIMATE, WINDOWS 7 PROFESSIONAL, REFERENCE-HW:SIMATIC S7-300/400",538,"TEM",1,"Simatic",0.23100000000000001,0]
["6ES78400CC042YN8","SIMATIC S7, S7-PDIAG V5.3 UNLOCK COPY LICENSE, ONLY VALID COMBINED WITH UNLOCK COPY LICENSE CONTRACT AND VALID LICENSE",485,"TEM",1,"Simatic",0.2,0]
["6ES78410CA010YX2","SIMATIC S7, S7-PLCSIM SOFTWARE UPDATE SERVICE WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE",105,"TEM",1,"Simatic",0.1,0]
["6ES78410CC002YX0","SIMATIC S7, S7-PLCSIM EPL-MASTER, ROYALTY-DUTY PER 1 INSTALLATION, ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT E-SW, SW AND DOCU. ON CD, LICENSE KEY ON CD/FD; CLASS A",364,"TEM",1,"Simatic",0.25,0]
["6ES78410CC002YX1","SIMATIC S7, S7-PLCSIM EPL-ROYALTY, SINGLE LICENSE F.1 INSTALLATION E-SW, WITHOUT SW AND DOCU. CLASS A ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",502,"TEM",1,"Simatic",0.05,0]
["6ES78410CC002YX2","SIMATIC S7, S7-PLCSIM EPL-MAINTENANCE, MAINTENANCE CHARGE F. ROYALTY FOR 12 MONTHS ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",105,"TEM",1,"Simatic",0.02,0]
["6ES78410CC050YA5","SIMATIC S7, S7-PLCSIM V5.4 FLOATING LICENSE FOR 1 USER E-SW, SW AND DOCU. ON CD, LICENSE KEY ON USB STICK, CLASS A,5 LANGUAGES(G,E,F,I,S), AS OF STEP7 V5.4 SP4 OR SP5 OR STEP7  V5.5 WITH OR W/O SP1, WINXPPROF, WIN 7 PROF/ULTIMATE, REFERENCE-HW:PG/PC",502,"TEM",1,"Simatic",0.214,0]
["6ES78410CC050YE5","SIMATIC S7, S7-PLCSIM V5.4 UPGRADE, FLOATING LICENSE FOR 1 USER E-SW, SW AND DOCU. ON CD, LICENSE KEY ON USB STICK, CLASS A,5 LANGUAGES(G,E,F,I,S), AS OF STEP7 V5.4 SP4 OR SP5 OR STEP7  V5.5 WITH OR W/O SP1, WINXPPROF, WIN 7 PROF/ULTIMATE, REFERENCE-HW:PG/PC",177,"TEM",1,"Simatic",0.214,0]
["6ES78410CC052YA0","SIMATIC S7, S7-PLCSIM V5.4, UNLOCK COPY LICENSE (UCL), BASIC PACKAGE FOR 20 INSTALLATIONS ONLY VALID COMBINED WITH UNLOCK COPY LICENSE CONTRACT",6022,"TEM",1,"Simatic",0.23499999999999999,0]
["6ES78410CC052YB0","SIMATIC S7, S7-PLCSIM V5.4, UNLOCK COPY LICENSE (UCL), ADDITIONAL PACKAGE FOR 5 INSTALLATIONS ONLY VALID COMBINED WITH UNLOCK COPY LICENSE CONTRACT; REQUIRES UCL BASIC PACKAGE",1506,"TEM",1,"Simatic",0.1,0]
["6ES78520CC010YA5","SIMATIC D7-SYS V7.0 FLOATING LICENSE F. 1 INSTALL., E-SW, SW AND DOCU ON CD, CLASS A, 2 LANGUAGES (G, E), RUNS UNDER 2000/XP, REFERENCE-HARDWARE: SIMATIC FM 458, T400, SIMATIC TDC, SIMADYN D",2614,"TEM",1,"Simatic",0.23400000000000001,0]
["6ES78520CC010YE5","SIMATIC D7-SYS V7.0 UPGRADE FROM RELEASE 5.X, FLOATING LICENSE F. 1 INSTALL., E-SW, SW AND DOKU ON CD, CLASS A, 2 LANGUAGES (G, E), RUNS UNDER WIN2000/XP, REFERENCE-HARDWARE: SIMATIC FM 458, T400, SIMATIC TDC, SIMADYN D",515,"TEM",1,"Simatic",0.23400000000000001,0]
["6ES78520CC010YL5","SIMATIC D7-SYS SOFTWARE UPDATE SERVICE WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE",380,"TEM",1,"Simatic",0.2,0]
["6ES78520CC020YA5","SIMATIC D7-SYS V7.1 FLOATING LICENSE F. 1 INSTALL., E-SW, SW AND DOCU ON CD, CLASS A, 2 LANGUAGES (G, E), RUNS UNDER 2000/XP, REFERENCE-HARDWARE: SIMATIC FM 458, T400, SIMATIC TDC, SIMADYN D",2614,"TEM",1,"Simatic",0.23699999999999999,0]
["6ES78520CC020YE5","SIMATIC D7-SYS V7.1 UPGRADE FROM RELEASE 5.X, FLOATING LICENSE F. 1 INSTALL., E-SW, SW AND DOKU ON CD, CLASS A, 2 LANGUAGES (G, E), RUNS UNDER WIN2000/XP, REFERENCE-HARDWARE: SIMATIC FM 458, T400, SIMATIC TDC, SIMADYN D",515,"TEM",1,"Simatic",0.23699999999999999,0]
["6ES78520CC020YN5","SIMATIC D7-SYS V7.1 UCL UNLOCK COPY LICENCE, ONLY VALID COMBINED WITH UNLOCK COPY LICNECE CONTRACT AND VALID LICENCES ACCORDING TO THE NUMBER OF USERS",371,"TEM",1,"Simatic",0.2,0]
["6ES78520CC030YA5","SIMATIC D7-SYS V8.0 FLOATING LICENSE F. 1 INSTALL., E-SW, SW AND DOCU ON CD, CLASS A, 2 LANGUAGES (G, E), EXECUTABLE UNDER WINXP, WIN7, REFERENCE-HARDWARE: SIMATIC FM 458, T400, SIMATIC TDC, SIMADYN D",2614,"TEM",1,"Simatic",0.23499999999999999,0]
["6ES78520CC030YE5","SIMATIC D7-SYS V8.0 UPGRADE FROM RELEASE 7.X, FLOATING LICENSE F. 1 INSTALL., E-SW, SW AND DOKU ON CD, CLASS A, 2 LANGUAGES (G, E), EXECUTABLE UNDER WINXP, WIN7, REFERENCE-HARDWARE: SIMATIC FM 458, T400, SIMATIC TDC, SIMADYN D",515,"TEM",1,"Simatic",0.22900000000000001,0]
["6ES78520CC040YA5","SIMATIC D7-SYS V8.1 INCL. D7-FB-GEN, FLOATING LICENSE F. 1 INSTALL., E-SW, SW AND DOCU ON CD, CLASS A, 2 LANGUAGES (G, E), EXECUTABLE UNDER WINXP, WIN7, REFERENCE-HARDWARE: SIMATIC FM 458, T400, SIMATIC TDC",3019,"TEM",1,"Simatic",0.23499999999999999,0]
["6ES78520CC040YE5","SIMATIC D7-SYS V8.1 INCL. D7-FB-GEN, UPGRADE FROM V8.X, FLOATING LICENSE F. 1 INSTALL., E-SW, SW AND DOKU ON CD, CLASS A, 2 LANGUAGES (G, E), EXECUTABLE UNDER WINXP, WIN7, REFERENCE-HARDWARE: SIMATIC FM 458, T400, SIMATIC TDC",604,"TEM",1,"Simatic",0.23400000000000001,0]
["6ES78530AA000YA5","SIEMENS Network Planner V1.0 Floating License; Software for simulation of PROFINET networks; software and documentation on DVD; license key on USB-STick; class A; 2 languages: GE,EN; executable under Windows 7 (32 BIT, 64 BIT)",1081,"TEM",1,"Simatic",0.22700000000000001,0]
["6ES78530AE000YA5","SIEMENS Network Planner V1.0 Floating License download; Software for simulation of PROFINET networks; software, documentation and license key for download; class A; 2 languages: GE,EN; executable under Windows 7 (32 BIT, 64 BIT) ******************************* email address is mandatory for delivery",1029,"TEM",1,"Simatic",1E-3,0]
["6ES78601AA004YX0","SIMATIC S7,TRAINERPACKAGE PID MODULUAR, SINGLE LICENSE F.6 INSTALLATION R-SW, SW AND DOCU. ON CD, LICENSE KEY ON FD, CLASS A, 2 LANGUAGES (G,E), EXECUTABLE UNDER WIN95/98/NT; REFERENCE-HW:SIMATIC S7-300/400 FOR EDUCATIONAL PURPOSES ONLY",1454,"TEM",1,"Simatic",1.1000000000000001,0]
["6ES78601AA100YX0","SIMATIC S7,MOD.PID CTRL,FB V5.1 SINGLE LICENSE F.1 INSTALLATION R-SW, SW AND DOCU. ON CD, CLASS A, 2 LANGUAGES (G,E), REFERENCE-HW: S7-300/-400, C7",798,"TEM",1,"Simatic",0.21,0]
["6ES78601AA100YX1","SIMATIC S7,MOD.PID CTRL,FB V5.1 SINGLE LICENSE F.1 INSTALLATION R-SW, WITHOUT SW AND DOCU., CLASS A, 2 LANGUAGES (G,E), REFERENCE-HW: S7-300/-400, C7",160,"TEM",1,"Simatic",1.9E-2,0]
["6ES78601AA102YE1","SIMATIC S7, MOD.PID CTRL V5.1 FB, EPL-ROYALTY, SINGLE LICENSE F.1 INSTALLATION R-SW WITHOUT SW AND DOCU., CLASS A, 2 LANGUAGES (G,E), REFERENCE-HW: S7-300/-400, C7 ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",160,"TEM",1,"Simatic",0.01,0]
["6ES78601XA010XB0","SIMATIC S7 PID PROFESSIONAL RUNTIME SINGLE LICENSE, W/O SOFTWARE AND DOCUMENTATION CLASS A, REFERENCE-HW: S7-300/400/WINAC",150,"TEM",1,"Simatic",1.2E-2,0]
["6ES78601XA010XH5","SIMATIC S7 PID PROFESSIONAL LICENSE KEY DOWNLOAD, FLOATING LICENSE FROM V11 W/O SOFTWARE AND DOCUMENTATION, CLASS A, REQUIRES STEP 7 PROFESSIONAL V1X REFERENCE-HW: S7-300/400/WINAC ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY",804,"TEM",1,"Simatic",1.4999999999999999E-2,0]
["6ES78601XA010XK5","SIMATIC S7 PID PROFESSIONAL LICENSE KEY DOWNLOAD UPGRADE LICENSE STANDARD PID CONTROL/ MODULAR PID CONTROL-> PID PROFESSIONAL FROM V11 W/O SOFTWARE AND DOCUMENTATION, CLASS A, REQUIRES STEP 7 PROFESSIONAL V1X REFERENCE-HW: S7-300/400/WINAC ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY",115,"TEM",1,"Simatic",1.4999999999999999E-2,0]
["6ES78601XA020XA5","SIMATIC S7 PID PROFESSIONAL FOR TIA PORTAL, FLOATING LICENSE FROM V11, RUNTIME SINGLE LICENSE, W/O SOFTWARE AND DOCUMENTATION, LICENSE KEY ON USB STICK, CLASS A, REQUIRES STEP 7 PROFESSIONAL V1X REFERENCE-HW: S7-300/400/WINAC",994,"TEM",1,"Simatic",0.251,0]
["6ES78601XA020XE5","SIMATIC S7 PID PROFESSIONAL FOR TIA PORTAL, UPGRADE LICENSE STANDARD PID CONTROL/ MODULAR PID CONTROL FROM V5.1-> PID PROFESSIONAL FROM V11 RUNTIME LICENSE W/O SOFTWARE AND DOCUMENTATION LICENSE KEY ON USB STICK, CLASS A, REQUIRES STEP 7 PROFESSIONAL V1X REFERENCE-HW: S7-300/400/WINAC",298,"TEM",1,"Simatic",0.16200000000000001,0]
["6ES78602AA004YX0","SIMATIC S7,TRAINERPACKAGE PID STANDARD, SINGLE LICENSE F.6 INSTALLATION R-SW, SW AND DOCU. ON CD, LICENSE KEY ON FD, CLASS A, 2 LANGUAGES (G,E), EXECUTABLE UNDER WIN95/98/NT; REFERENCE-HW:SIMATIC S7-300/400 FOR EDUCATIONAL PURPOSES ONLY",1454,"TEM",1,"Simatic",1.1000000000000001,0]
["6ES78602AA210YX0","SIMATIC S7, STAND.PID CTRL V5.2 SINGLE LICENSE F.1 INSTALLATION R-SW, SW AND DOCU. ON CD, CLASS A, 2 LANGUAGES (G,E), REFERENCE-HW: S7-300/-400, C7",637,"TEM",1,"Simatic",0.21,0]
["6ES78602AA210YX1","SIMATIC S7, STAND.PID CTRL V5.2 SINGLE LICENSE F.1 INSTALLATION R-SW, WITHOUT SW AND DOCU., CLASS A, 2 LANGUAGES (G,E), REFERENCE-HW: S7-300/-400, C7",128,"TEM",1,"Simatic",1.4E-2,0]
["6ES78604AA010YX0","SIMATIC S7, PID SELF TUNER V5.1 SINGLE LICENSE F.1 INSTALLATION R-SW, SW AND DOCU. ON CD, CLASS A, 2 LANGUAGES (G,E), REFERENCE-HW: S7-300/-400, C7",297,"TEM",1,"Simatic",0.223,0]
["6ES78604AA010YX1","SIMATIC S7, PID SELF TUNER V5.1 SINGLE LICENSE F.1 INSTALLATION R-SW, WITHOUT SW AND DOCU., CLASS A, 2 LANGUAGES (G,E), REFERENCE-HW: S7-300/-400, C7",59.300000000000004,"TEM",1,"Simatic",8.9999999999999993E-3,0]
["6ES78620AC010YA0","SIMATIC S7, SW REDUNDANCY V1.2 SINGLE LICENSE F.1 INSTALLATION R-SW (FOR TWO CPU), SW AND DOCU. ON CD, CLASS A,5 LANGUAGES(G,E,F,I,S), EXECUTABLE UNDER WIN95/98/ME/ WINNT/2000PROF, REFERENCE-HW:SIMATIC S7-300/400 FROM CPU 315",663,"TEM",1,"Simatic",0.21299999999999999,0]
["6ES78620AC010YA1","SIMATIC S7, SW REDUNDANCY V1.2 SINGLE LICENSE F.1 INSTALLATION R-SW, WITHOUT SW AND DOCU., CLASS A,5 LANGUAGES(G,E,F,I,S), EXECUTABLE UNDER WIN95/98/ME/ WINNT/2000PROF, REFERENCE-HW:SIMATIC S7-300/400 FROM CPU 315",532,"TEM",1,"Simatic",0.02,0]
["6ES78640AC010YX0","SIMATIC S7,EASY MOTION CTRL 2.1 SINGLE LICENSE F.1 INSTALLATION R-SW, SW AND DOCU. ON CD, CLASS A, 2 LANGUAGES (G,E), EXECUTABLE UNDER STEP7 FROM V5.3 SP2, REFERENCE-HW: SIMATIC S7-300/400/WINAC",473,"TEM",1,"Simatic",0.20599999999999999,0]
["6ES78640AF010YX0","SIMATIC S7, EASY MOTION CONTROL RUNTIME SINGLE LICENSE  W/O SOFTWARE AND DOCUMENTATION CLASS A, REFERENCE-HW: S7-300/400/WINAC",320,"TEM",1,"Simatic",1.2E-2,0]
["6ES78641CC002YP0","SIMATIC S7, S7-TECHNOLOGY OPTIONAL PACKAGE FOR STEP7 V5.5 SP1 (OR HIGHER), EPL-MASTER, ROYALTY-DUTY PER 1 INSTALLATION, ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT E-SW, SW AND DOCU. ON CD, LICENSE KEY ONF CD/FD; CLASS A",330,"TEM",1,"Simatic",0.2,0]
["6ES78641CC420XH5","SIMATIC S7, S7-TECHNOLOGY V4.2, OPTIONAL PACKAGE FOR STEP7, LICENSE KEY DOWNLOAD, FLOATING LICENSE FOR 1 USER, FOR CONFIGURING AND PROGRAMMING OF TECHNOLOGY USER PROGRAMS CLASS A, EXECUTABLE UNDER WINDOWS XP (32 BIT), WINDOWS 7 (32/64 BIT), REFERENCE-HW: S7-315T, S7-317T, S7-317TF, MICROBOX 420-T, ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY!",427,"TEM",1,"Simatic",1E-3,0]
["6ES78641CC420YA5","SIMATIC S7, S7-TECHNOLOGY V4.2 INCL. LATEST SERVICE PACK, OPTIONAL PACKAGE FOR STEP7 FOR CONFIGURING AND PROGRAMMING OF TECHNOLOGY USER PROGRAMS FLOATING LICENSE FOR 1 USER, E-SW, SW AND DOCU. ON DVD, LICENSE KEY ON USB STICK, CLASS A, 4 LANGUAGES (GE,EN,FR,IT), EXECUTABLE UNDER WINDOWS 7 (32/64 BIT), REFERENCE-HW: S7-315T, S7-317T, S7-317TF, MICROBOX 420-T",461,"TEM",1,"Simatic",0.318,0]
["6ES78641CC420YA7","SIMATIC S7, S7-TECHNOLOGY V4.2 INCL. LATEST SERVICE PACK, TRIAL VERSION, FOR CONFIGURING AND PROGRAMMING OF TECHNOLOGY USER PROGRAMS DATA MEDIUM INCL. TRIAL LICENSE FOR 14 DAYS, E-SW, SW AND DOCU. ON DVD, LICENSE KEY ON USB STICK, CLASS A, 4 LANGUAGES (GE,EN,FR,IT), EXECUTABLE UNDER WINDOWS 7 (32/64 BIT), REFERENCE-HW: S7-315T, S7-317T, S7-317TF, MICROBOX 420-T",29,"TEM",1,"Simatic",0.316,0]
["6ES78641CC420YE5","SIMATIC S7, S7-TECHNOLOGY V4.2 UPGRADE (V4.1.X TO V4.2), INCL. LATEST SERVICE PACK, FOR CONFIGURING AND PROGRAMMING OF TECHNOLOGY USER PROGRAMS FLOATING LICENSE FOR 1 USER, E-SW, SW AND DOCU. ON DVD, LICENSE KEY ON USB STICK, CLASS A, 4 LANGUAGES (GE,EN,FR,IT), EXECUTABLE UNDER WINDOWS 7 (32/64 BIT), REFERENCE-HW: S7-315T, S7-317T, S7-317TF, MICROBOX 420-T",143,"TEM",1,"Simatic",0.316,0]
["6ES78642XA010XH5","SIMATIC S7, EASY MOTION CONTROL LICENSE KEY DOWNLOAD FLOATING LICENSE FROM V11 W/O SOFTWARE AND DOCUMENTATION CLASS A, REQUIRES STEP 7 PROFESSIONAL V1X REFERENCE-HW: S7-300/400/WINAC ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY",140,"TEM",1,"Simatic",1.4999999999999999E-2,0]
["6ES78642XA020XA5","SIMATIC S7 EASY MOTION CONTROL FOR TIA PORTAL, FLOATING LICENSE FROM V11 W/O SOFTWARE AND DOCUMENTATION LICENSE KEY ON USB STICK, CLASS A, REQUIRES STEP 7 PROFESSIONAL V1X REFERENCE-HW: S7-300/400/WINAC",450,"TEM",1,"Simatic",0.14799999999999999,0]
["6ES78701AA010YA0","SIMATIC S7, MODBUS MASTER  V3.1 SINGLE LICENSE F.1 INSTALLATION R-SW, SW AND DOCU. ON CD, HW-DONGLE, CLASS A, 3 LANGUAGES (G,E,F), EXECUTABLE U. STEP7 FROM V4.2, REFERENCE-HW: CP341 AND CP441-2",1323,"TEM",1,"Simatic",0.21299999999999999,0]
["6ES78701AA010YA1","SIMATIC S7, MODBUS MASTER  V3.1 SINGLE LICENSE F.1 INSTALLATION R-SW, WITHOUT SW AND DOCU., HW-DONGLE, CLASS A, 3 LANGUAGES (G,E,F), EXECUTABLE U. STEP7 FROM V4.2, REFERENCE-HW: CP341 AND CP441-2",994,"TEM",1,"Simatic",3.9E-2,0]
["6ES78701AB010YA0","SIMATIC S7, MODBUS SLAVE V3.1 SINGLE LICENSE F.1 INSTALLATION R-SW, SW AND DOCU. ON CD, HW-DONGLE, CLASS A, 3 LANGUAGES (G,E,F), EXECUTABLE U. STEP7 FROM V4.2, REFERENCE-HW: CP341 AND CP441-2",1323,"TEM",1,"Simatic",0.217,0]
["6ES78701AB010YA1","SIMATIC S7, MODBUS SLAVE V3.1 SINGLE LICENSE F.1 INSTALLATION R-SW, WITHOUT SW AND DOCU., HW-DONGLE, CLASS A, 3 LANGUAGES (G,E,F), EXECUTABLE U. STEP7 FROM V4.2, REFERENCE-HW: CP341 AND CP441-2",994,"TEM",1,"Simatic",3.7999999999999999E-2,0]
["6ES79005AA000XA0","SIMATIC PG, SUPPLY CABLE 3M FOR FIELD PG M5/M4/M2 FOR GERMANY; FRANCE; SPAIN; NETHERLANDS; BELGIUM; SWEDEN; AUSTRIA; FINLAND",12.100000000000001,"TEM",1,"Simatic",0.247,1]
["6ES79005BA000XA0","SIMATIC PG, SUPPLY CABLE 3M FOR FIELD PG M5/M4/M2 FOR UNITED KINGDOM",12.100000000000001,"TEM",1,"Simatic",0.27500000000000002,1]
["6ES79005CA000XA0","SIMATIC PG, SUPPLY CABLE 3M FOR FIELD PG M5/M4/M2 FOR SWITZERLAND",12.100000000000001,"TEM",1,"Simatic",0.23100000000000001,1]
["6ES79005DA000XA0","SIMATIC PG, SUPPLY CABLE 3M FOR FIELD PG M5/M4/M2 FOR USA",12.100000000000001,"TEM",1,"Simatic",0.224,1]
["6ES79005EA000XA0","SIMATIC PG, SUPPLY CABLE 3M FOR FIELD PG M5/M4/M2 FOR ITALY",12.100000000000001,"TEM",1,"Simatic",0.22500000000000001,1]
["6ES79005FA000XA0","SIMATIC PG, SUPPLY CABLE 3M FOR FIELD PG M4/M2 FOR CHINA",12.100000000000001,"TEM",1,"Simatic",0.23699999999999999,1]
["6ES79010BF000AA0","SIMATIC S7, MPI CABLE FOR CONNECTING SIMATIC S7 AND PG VIA MPI 5M",29.6,"TEM",1,"Simatic",0.25800000000000001,1]
["6ES79011BF000XA0","SIMATIC S7,CONNECTING CABLE FOR HMI ADAPTER AND PC/TS ADAPTER, (RS232 / ZERO MODEM CABLE), 6 M",21.400000000000002,"TEM",1,"Simatic",0.25900000000000001,0]
["6ES79014BD000XA0","SIMATIC DP, CONNECTION CABLE F. PROFIBUS, 12 MBAUD, F. CONN. A PG TO PROFUBUS DP, PRECUT A. PREASSEMBLED WITH 2 X 9-PIN SUB-D CONNECTOR, 3 M",104,"TEM",1,"Simatic",0.315,1]
["6ES79021AB000AA0","SIMATIC S7/M7, CABLE FOR POINT TO POINT CONNECTIONS RS232C - RS232C, 9-POLE SUBMIN. D SOCKETS, 5 M LENGTH",85.4,"TEM",1,"Simatic",0.25700000000000001,0]
["6ES79021AC000AA0","SIMATIC S7/M7, CABLE FOR POINT TO POINT CONNECTIONS RS232C - RS232C, 9-POLE SUBMIN. D SOCKETS, 10 M LENGTH",107,"TEM",1,"Simatic",0.44900000000000001,0]
["6ES79021AD000AA0","SIMATIC S7/M7, CABLE FOR POINT TO POINT CONNECTIONS RS232C - RS232C, 9-POLE SUBMIN. D SOCKETS, 15 M LENGTH",121,"TEM",1,"Simatic",0.65500000000000003,0]
["6ES79022AB000AA0","SIMATIC S7/M7, CABLE FOR POINT TO POINT CONNECTIONS TTY - TTY, 9-POLE SUBMIN.D PINS 5 M",85.4,"TEM",1,"Simatic",0.20100000000000001,0]
["6ES79022AC000AA0","SIMATIC S7/M7, CABLE FOR POINT TO POINT CONNECTIONS TTY - TTY, 9-POLE SUBMIN.D PINS 10 M",107,"TEM",1,"Simatic",0.34899999999999998,0]
["6ES79022AG000AA0","SIMATIC S7/M7, CABLE FOR POINT TO POINT CONNECTIONS TTY - TTY, 9-POLE SUBMIN.D PINS 50 M",185,"TEM",1,"Simatic",1.5980000000000001,0]
["6ES79023AB000AA0","SIMATIC S7/M7, CABLE FOR POINT TO POINT CONNECTIONS RS422 - RS422, 15-POLE SUBMIN. D PINS, 5 M LENGTH",85.4,"TEM",1,"Simatic",0.247,0]
["6ES79023AC000AA0","SIMATIC S7/M7, CABLE FOR POINT TO POINT CONNECTIONS RS422 - RS422, 15-POLE SUB-D PINS, LENGTH 10 M",107,"TEM",1,"Simatic",0.43099999999999999,0]
["6ES79023AG000AA0","SIMATIC S7/M7, CABLE FOR POINT TO POINT CONNECTIONS RS422 - RS422, 15-POLE SUBMIN. D PINS, 50 M",185,"TEM",1,"Simatic",1.9870000000000001,0]
["6ES79120AA000AA0","SIMATIC S7, SLOT NUMBER LABELS",7.1000000000000005,"TEM",1,"Simatic",6.0000000000000001E-3,0]
["6ES79538LF310AA0","SIMATIC S7, MICRO MEMORY CARD FOR S7-300/C7/ET 200, 3.3 V NFLASH, 64 KB",39.900000000000006,"TEM",1,"Simatic",0.03,1]
["6ES79538LG310AA0","SIMATIC S7, MICRO MEMORY CARD FOR S7-300/C7/ET 200, 3.3 V NFLASH, 128 KB",76.5,"TEM",1,"Simatic",0.03,1]
["6ES79538LJ310AA0","SIMATIC S7, MICRO MEMORY CARD F. S7-300/C7/ET 200, 3.3 V NFLASH, 512 KB",182,"TEM",1,"Simatic",0.03,1]
["6ES79538LL310AA0","SIMATIC S7, MICRO MEMORY CARD P. S7-300/C7/ET 200, 3.3 V NFLASH, 2 MBYTES",261,"TEM",1,"Simatic",0.03,1]
["6ES79538LM310AA0","SIMATIC S7, MICRO MEMORY CARD FOR S7-300/C7/ET 200, 3.3 V NFLASH, 4 MB",319,"TEM",1,"Simatic",0.03,1]
["6ES79538LP310AA0","SIMATIC S7, MICRO MEMORY CARD FOR S7-300/C7/ET 200, 3.3 V NFLASH, 8 MB",397,"TEM",1,"Simatic",0.03,1]
["6ES79548LC020AA0","SIMATIC S7, MEMORY CARD FOR S7-1X00 CPU/SINAMICS, 3,3 V FLASH, 4 MBYTE",53.6,"TEM",1,"S7-1200",0.03,1]
["6ES79548LE020AA0","SIMATIC S7, MEMORY CARD FOR S7-1X00 CPU/SINAMICS, 3,3 V FLASH, 12 MBYTE",177,"TEM",1,"S7-1200",0.03,1]
["6ES79548LF020AA0","SIMATIC S7, MEMORY CARD FOR S7-1X00 CPU/SINAMICS, 3,3 V FLASH, 24 MBYTE",268,"TEM",1,"S7-1200",3.1E-2,1]
["6ES79548LL020AA0","SIMATIC S7, MEMORY CARD FOR S7-1X00 CPU, 3,3 V FLASH, 256 MBYTE",368,"TEM",1,"S7-1200",3.1E-2,1]
["6ES79548LP020AA0","SIMATIC S7, MEMORY CARD FOR S7-1X00 CPU, 3,3 V FLASH, 2 GBYTE",683,"TEM",1,"S7-1200",3.1E-2,1]
["6ES79548LT020AA0","SIMATIC S7, MEMORY CARD FOR S7-1X00 CPU, 3,3 V FLASH, 32 GBYTE",1048,"TEM",1,"S7-1200",3.1E-2,1]
["6ES79711AA000AA0","SIMATIC S7, BACKUP BATTERY (LI) 3.6V/MIN. 0.85AH, FOR FOR S7-300 CPUS AND S5-90U",14.100000000000001,"TEM",1,"Simatic",1.2E-2,1]
["6ES79715BB000AA0","SIMATIC S7-300, SUPERCAP FOR THE BACKUP OF THE REAL-TIME CLOCK FROM CPU 314 AND UPWARDS",32.5,"TEM",1,"Simatic",8.0000000000000002E-3,1]
["6ES79720AA020XA0","SIMATIC DP, RS485 REPEATER FOR THE CONNECTION OF PROFIBUS/MPI BUS SYSTEMS WITH MAX. 31 NODES; MAX. 12 MBIT/S, DEGREE OF PRO- TECTION IP20 IMPROVED USABILITY",320,"TEM",1,"Simatic",0.248,1]
["6ES79720AB010XA0","SIMATIC S7, DIAGNOSIS-REPEATER FOR PROFIBUS DP, FOR ONLINE PROFIBUS CABLE DIAGNOSTICS, DP-STANDARD SLAVE TO 12MBIT/S, DEGREE OF PROTECTION IP20, FAST-CONNECT TECHNOLOGY",768,"TEM",1,"Simatic",0.32200000000000001,1]
["6ES79720BA120XA0","SIMATIC DP, BUS CONNECTOR FOR PROFIBUS UP TO 12 MBIT/S 90 DEGREE ANGLE OUTGOING CABLE, 15,8 X 64 X 35,6 MM (WXHXD), TERMINAT. RESIST. WITH ISOLAT. FUNCTION, WITHOUT PG SOCKET",40.200000000000003,"TEM",1,"Simatic",0.05,1]
["6ES79720BA300XA0","SIMATIC DP, BUS CONNECTOR FOR PROFIBUS WITH TILTED CABLE OUTLET,  MAX.1.5 MBIT/S, INSUL.PIERCING CONN.DEV., 15 X 57,6 X 39,5 MM (WXHXD), W/O LAN TERMINAT.RESIST. AND.PG CONNECTION SOCKET",23.400000000000002,"TEM",1,"Simatic",4.2999999999999997E-2,1]
["6ES79720BA420XA0","SIMATIC DP,BUS CONNECTOR FOR PROFIBUS UP TO 12 MBIT/S WITH TILTED CABLE OUTLET, 15,8 X 54 X 39,5 MM (WXHXD), TERMINAT. RESIST. WITH ISOLAT. FUNCTION, WITHOUT PG SOCKET",40.200000000000003,"TEM",1,"Simatic",4.2999999999999997E-2,1]
["6ES79720BA520XA0","SIMATIC DP,BUS CONNECTOR FOR PROFIBUS UP TO 12 MBIT/S 90 DEGREE ANGLE CABLE OUTLET, IPCD TECHOLOGY FAST CONNECT, WITHOUT PG SOCKET 15,8 X 59 X 35,6 MM (WXHXD),",40.200000000000003,"TEM",1,"Simatic",4.2999999999999997E-2,1]
["6ES79720BA520XB0","SIMATIC DP,BUS CONNECTOR FOR PROFIBUS UP TO 12 MBIT/S 90 DEGREE ANGLE CABLE OUTLET, 15,8 X 59 X 35,6 MM (WXHXD), IPCD TECHOLOGY FAST CONNECT, WITHOUT PG SOCKET 100 PIECES PER PACKAGING UNIT",3914,"ΠΑΚ",1,"Simatic",3.2130000000000001,0]
["6ES79720BA610XA0","SIMATIC DP, BUS CONNECTOR FOR PROFIBUS UP TO 12 MBIT/S 35 DEGREE ANGLE CABLE OUTLET, IPCD TECHOLOGY FAST CONNECT, WITHOUT PG SOCKET 15,8 X 54 X 39,5 MM (WXHXD),",40.200000000000003,"TEM",1,"Simatic",4.4999999999999998E-2,1]
["6ES79720BA700XA0","SIMATIC DP, BUS CONNECTOR FOR PROFIBUS UP TO 12 MBIT/S 90 DEGREE ANGLE CABLE OUTLET, 15.8 X 72.2 X 36.4 MM (WXHXD), IPCD TECHOLOGY FAST CONNECT, WITHOUT PG SOCKET",40.200000000000003,"TEM",1,"Simatic",4.7E-2,1]
["6ES79720BB120XA0","SIMATIC DP, BUS CONNECTOR FOR PROFIBUS UP TO 12 MBIT/S 90 DEGREE ANGLE CABLE OUTLET, 15,8 X 64 X 35,6 MM (WXHXD), TERMINAT. RESIST. WITH ISOLAT. FUNCTION, WITH PG SOCKET",52.400000000000006,"TEM",1,"Simatic",0.06,1]
["6ES79720BB420XA0","SIMATIC DP, BUS CONNECTOR FOR PROFIBUS UP TO 12 MBIT/S WITH TILTED CABLE OUTLET, 15,8 X 54 X 39,5 MM (WXHXD), TERMINAT. RESIST. WITH ISOLAT. FUNCTION, WITH PG SOCKET",52.400000000000006,"TEM",1,"Simatic",4.7E-2,1]
["6ES79720BB520XA0","SIMATIC DP,BUS CONNECTOR FOR PROFIBUS UP TO 12 MBIT/S 90 DEGREE ANGLE CABLE OUTLET, IPCD TECHOLOGY FAST CONNECT, WITH PG SOCKET 15,8 X 59 X 35,6 MM (WXHXD),",52.400000000000006,"TEM",1,"Simatic",4.7E-2,1]
["6ES79720BB520XB0","SIMATIC DP,BUS CONNECTOR FOR PROFIBUS UP TO 12 MBIT/S 90 DEGREE ANGLE OUTGOING CABLE, 15,8 X 59 X 35,6 MM (WXHXD), IPCD TECHOLOGY FAST CONNECT, WITH PG SOCKET 100 PIECES PER PACKAGING UNIT",5218,"ΠΑΚ",1,"Simatic",3.734,0]
["6ES79720BB610XA0","SIMATIC DP, BUS CONNECTOR FOR PROFIBUS UP TO 12 MBIT/S 35 DEGREE ANGLE CABLE OUTLET, IPCD TECHOLOGY FAST CONNECT, WITH PG SOCKET 15,8 X 54 X 39,5 MM (WXHXD),",52.400000000000006,"TEM",1,"Simatic",0.05,1]
["6ES79720BB700XA0","SIMATIC DP,BUS CONNECTOR FOR PROFIBUS UP TO 12 MBIT/S 90 DEGREE ANGLE CABLE OUTLET, 15,8 X 72,2 X 36,4 MM (WXHXD), IPCD TECHOLOGY FAST CONNECT, WITH PG SOCKET",52.400000000000006,"TEM",1,"Simatic",5.0999999999999997E-2,1]
["6ES79720DA000AA0","SIMATIC DP, RS485 RESISTOR FOR TERMINATING PROFIBUS-/MPI-NETWORKS",79.600000000000009,"TEM",1,"Simatic",0.105,1]
["6ES79724AA020XA0","SIMATIC DP, POWER RAIL BOOSTER SIGNAL AMPLIFIER FOR TRANSMITTING THE PROTOCOL OF PROFIBUS-DP USING COLLECTOR WIRES, MAX 500 KBIT/S",797,"TEM",1,"Simatic",0.51200000000000001,1]
["6ES79724AA500XA0","SIMATIC DP, PRB SEGMENT CONTROLLER, AUTOMATIC CHANGE-OVER SWITCH BETWEEN PRB SEGMENTS",672,"TEM",1,"Simatic",0.83699999999999997,1]
["6ES79731GC000AA0","SIMATIC S7-300, FUSE SET 6,3A FOR SM 322 6ES7322-1CF00-0AA0 10 PIECES PER PACKAGING UNIT",23.3,"ΠΑΚ",1,"Simatic",3.4000000000000002E-2,1]
["6ES79731HD000AA0","SIMATIC S7, FUSE SET FOR 6ES7322-1FF01-0AA0 AND 6ES7322-1FH00-0AA0: 10 FUSES 8A RAPID, 2 FUSE HOLDERS",30.400000000000002,"TEM",1,"Simatic",2.3E-2,1]
["6ES79740AA000AA0","SIMATIC S7, MEAS. RANGE MODULES FOR ANALOG INPUTS, 2 PIECES PER PACKAGING UNIT",20.8,"ΠΑΚ",1,"Simatic",1.2999999999999999E-2,1]
["6ES79971BA004AX2","SIEMENS SOLUTION PARTNER STEP7 PROFESSIONAL SUS SOFTWARE UPDATE SERVICE",158,"TEM",1,"Simatic",0.1,0]
["6ES79971BB004AX0","SIEMENS SOLUTION PARTNER STEP7 PROFESSIONAL STANDARD SOFTWARE",788,"TEM",1,"Simatic",0.4,0]
["6ES79971BB004AX5","SIEMENS SOLUTION PARTNER STEP7 POWER PACK UPGRADE STEP7 TO STEP7 PROFESSIONAL",331,"TEM",1,"Simatic",0.4,0]
["6ES79971BC004AX0","SIEMENS SOLUTION PARTNER STEP7 PROFESSIONAL PLUS CONSISTS OF: CFC, S7-PDIAG",1064,"TEM",1,"Simatic",0.75,0]
["6ES79971BD004AX2","SIEMENS SOLUTION PARTNER STEP7 PROFESSIONAL PLUS SUS SOFTWARE UPDATE SERVICE  FOR STEP7 PROFESSIONAL PLUS",243,"TEM",1,"Simatic",0.1,0]
["6ES79971CA004BA0","SIEMENS SOLUTION PARTNER WELCOME / FOLLOW UP PACKAGE \"AUTOMATION\" CONSISTS OF A&D SOFTWARE ( PREMIUM STUDIO + SELECTED LICENSES) AUTOMATION VALUE CARD, ANUAL FEE FOR FOLLOW-UP SERVICE",525,"TEM",1,"Simatic",1.0369999999999999,0]
["6ES79971CA004BA1","SIEMENS VALUE ADDED RESELLER PARTNER WELCOME / FOLLOW UP VALUE PACKAGE \"SIMATIC FA/HMI\" CONSISTING OF: FA/HMI SOFTWARE (SELECTED LICENSES), AUTOMATION VALUE CARD, ANUAL FEE FOR FOLLOW-UP SERVICE",525,"TEM",1,"Simatic",3.6999999999999998E-2,0]
["6ES79971CA004BA2","SIEMENS VALUE ADDED RESELLER PARTNER WELCOME / FOLLOW UP VALUE PACKAGE MICRO AUTOMATION CONSISTING OF: MICRO AUTOMATION (MA) SOFTWARE (SELECTED LICENSES), AUTOMATION VALUE CARD, ANUAL FEE FOR FOLLOW-UP SERVICE",525,"TEM",1,"Simatic",3.6999999999999998E-2,0]
["6ES79971CA004BA3","SIEMENS PACKAGE APPROVED PARTNER AUTOMATION DRIVES WELCOME CONSISTING OF: WELCOME LETTER, DESIGN GUIDELINES, EMBLEM",105,"TEM",1,"Simatic",3.6999999999999998E-2,0]
["6ES79971CA004BA7","Siemens Package Solution Partner Automation Drives Welcome consiSTing of: Welcome letter, Design guidelines, Emblem",105,"TEM",1,"Simatic",1.0369999999999999,0]
["6ES79971CA004KA0","SIEMENS SOLUTION PARTNER WELCOME / FOLLOW UP PACKAGE \"AUTOMATION\" CONSISTS OF A&D SOFTWARE ( PREMIUM STUDIO + SELECTED LICENSES) AUTOMATION VALUE CARD, ANUAL FEE FOR FOLLOW-UP SERVICE INCL. CHINESE EXTENSION PACKAGE",525,"TEM",1,"Simatic",0.45,0]
["6ES79971CA007AA0","SIEMENS SOLUTION PARTNER PARTNER PLATE",94.5,"TEM",1,"Simatic",0.1,0]
["6ES79971CB044BA0","WELCOME PACKAGE MICRO AUTOMATION CONSISTING OF: 1 X S7-1200 CPU 1214C DC/DC/DC, 1 X STEP7 BASIC, SINGLE LIC., 1X ANALOG OUTPUT SB1232, 1 AO, 1 X POWER MODULE 2,5A, PM 1207, 1 X SWITCH MODULE CSM 1277, 1 X KTP700 BASIC COLOR PN 7\",  1 X LOGO! 12/24RCE, 1 X LOGO! SOFT COMFORT, SINGLE LIC., ******************************* FOR SOLUTION PARTNERS ONLY",817,"TEM",1,"Simatic",3,0]
["6ES79971CB404BA0","SIEMENS SOLUTION PARTNER WELCOME/FOLLOW UP PACKAGE AUTOMATION - OVERSEAS\" CONSISTS OF: A&D SOFTWARE (PREMIUM STUDIO AND SELECTED LICENSES)",315,"TEM",1,"Simatic",0.2,0]
["6ES79971CF104BA0","SIEMENS SOLUTION PARTNER FOLLOW UP PACKAGE \"SIEMENS RUSSIA GROUP 1\" CONSISTS OF: FOLLOW UP A&D SOFTWARE (PREMIUM STUDIO AND SELECTED LICENSES)",200,"TEM",1,"Simatic",0.1,0]
["6ES79971CF204BA0","SIEMENS SOLUTION PARTNER FOLLOW UP PACKAGE \"SIEMENS RUSSIA GROUP 2\" CONSISTS OF: FOLLOW UP A&D SOFTWARE (PREMIUM STUDIO AND SELECTED LICENSES)",504,"TEM",1,"Simatic",0.1,0]
["6ES79971CF304BA0","SIEMENS SOLUTION PARTNER FOLLOW UP PACKAGE \"SIEMENS RUSSIA GROUP 3\" CONSISTS OF: FOLLOW UP A&D SOFTWARE (PREMIUM STUDIO AND SELECTED LICENSES)",983,"TEM",1,"Simatic",0.1,0]
["6ES79971CF404BA0","SIEMENS SOLUTION PARTNER FOLLOW UP PACKAGE \"SIEMENS RUSSIA GROUP 4\" CONSISTS OF: FOLLOW UP A&D SOFTWARE (PREMIUM STUDIO AND SELECTED LICENSES)",1208,"TEM",1,"Simatic",0.1,0]
["6ES79971CF504BA0","SIEMENS SOLUTION PARTNER FOLLOW UP PACKAGE \"SIEMENS RUSSIA GROUP 5\" CONSISTS OF: FOLLOW UP A&D SOFTWARE (PREMIUM STUDIO AND SELECTED LICENSES)",1575,"TEM",1,"Simatic",0.1,0]
["6ES79971CF604BA0","SIEMENS SOLUTION PARTNER FOLLOW UP PACKAGE \"SIEMENS RUSSIA GROUP 6\" CONSISTS OF: FOLLOW UP A&D SOFTWARE (PREMIUM STUDIO AND SELECTED LICENSES)",2100,"TEM",1,"Simatic",0.1,0]
["6ES79971DA004BA0","SIEMENS SOLUTION PARTNER PARTNER FEE FOR PROGRAM MODULE \"AUTOMATION SYSTEM SIMATIC\", ANUAL FEE",525,"TEM",1,"Simatic",3.7999999999999999E-2,0]
["6ES79971DB004BA0","SIEMENS SOLUTION PARTNER PARTNER FEE FOR PROGRAM MODULE \"MICRO AUTOMATION\", ANUAL FEE",525,"TEM",1,"Simatic",0.2,0]
["6ES79971DG104BA0","SIEMENS SOLUTION PARTNER PARTNER FEE FOR PROGRAM MODULE \"WIND AUTOMATION SIMATIC\" ANUAL FEE",525,"TEM",1,"Simatic",0.1,0]
["6ES79988XC018YE0","SIMATIC MANUAL COLLECTION ON DVD, 5 LANGUAGES, ALL MANUALS ABOUT S7-1200/1500/200/300/400,LOGO!, SIMATIC DP, PC, PG, STEP7, ENGINEERING SW, RUNTIME SW, PCS7, SIMATIC HMI, SIMATIC NET, SIMATIC IDENT",112,"TEM",1,"Simatic",0.11799999999999999,0]
["6ES79988XC018YE2","SIMATIC MANUAL COLLECTION ON DVD, 5 LANGUAGES, SOFTWARE UPDATE SERVICE WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE",339,"TEM",1,"Simatic",0.4,0]
["6GK11820BB010AA1","PROFINET IO ASIC, ERTEC 200 (LEADFREE), 10/100 MBIT/S INDUSTRIAL ETHERNET, ASIC WITH ARM 946 PROZESSOR, 2-PORT SWITCH, PHY INTEGRATED, SINGLE-TRAY 70 PCS.",1552,"ΠΑΚ",1,"Simatic",0.48399999999999999,0]
["6GK11820BB010AA2","PROFINET IO ASIC, ERTEC 200 (LEADFREE), 10/100 MBIT/S INDUSTRIAL ETHERNET, ASIC WITH ARM 946 PROCESSOR, 2-PORT SWITCH, PHY INTEGRATED, DRYPACK (5 TRAYS) 350 PCS.",7184,"ΠΑΚ",1,"Simatic",1.321,0]
["6GK11828BB010AA2","PROFINET IO ASIC, SPNC021E20 (LEADFREE),10/100MBIT/S ASIC WITH ARM 946 PROCESSOR, 2-PORT-SWITCH, PHY INTEGRIERT, DRYPACK (5 TRAYS) 350 PIECES FOR INTERNAL USE ONLY",12000,"ΠΑΚ",1,"Simatic",1.331,0]
["6GK11840BB010AA1","PROFINET IO ASIC, ERTEC 400 (LEADFREE), 10/100 MBIT/S INDUSTRIAL ETHERNET, ASIC WITH ARM 946 PROCESSOR, 4-PORT SWITCH, PCI-INTERFACE, SINGLE-TRAY 70 PIECES",3756,"ΠΑΚ",1,"Simatic",0.48399999999999999,0]
["6GK11840BB010AA2","PROFINET IO ASIC, ERTEC 400 (LEADFREE), 10/100 MBIT/S INDUSTRIAL ETHERNET, ASIC WITH  ARM 946 PROCESSOR, 4-PORT-SWITCH, PCI-INTERFACE DRYPACK (5 TRAYS) 350 PIECES",17143,"ΠΑΚ",1,"Simatic",1.333,0]
["A5E00086045","SIMATIC PG, SPARE PART SERIAL PORT ADAPTERS D9/D25 FOR FIELD PG",2.6,"TEM",1,"Simatic",0.04,1]
["A5E00166133","SIMATIC PG, SPARE PART SET RUBBER FEET (10 PIECES) FOR FIELD PG",25.5,"ΠΑΚ",1,"Simatic",2.9000000000000001E-2,1]
["A5E00448516","PLUG-IN POWER SUPPLY UNIT FOR DK-ERTEC 200/400 PN IO CANNOT BE ORDERED SEPARATELY",81.7,"TEM",1,"Simatic",0.25,1]
["A5E00749366","SIMATIC PG, SPARE PART TOUCH PAD FOR FIELD PG",20,"TEM",1,"Simatic",0.1,1]
["A5E02237594","SIMATIC PG, SPARE PART, DVI-VGA-ADAPTER FOR FIELD PG M5/M4/M3",10.5,"TEM",1,"Simatic",1E-3,1]
["A5E02262046","SIMATIC PG, SPARE PART, HDD SLIDE IN FOR FIELD PG M5/M4/M3",26.3,"TEM",1,"Simatic",0.1,1]
["A5E02916227","SIMATIC PG, SPARE PART, COVER MEMORY CARD COVER, SPRING FOR FIELD PG M5/M4/M3 (20 PIECES EACH)",36.800000000000004,"TEM",1,"Simatic",1E-3,1]
["A5E02916228","SIMATIC PG, SPARE PART, DISPLAY LOCKING SLIDER, SPRING FOR FIELD PG M5/M4/M3 (20 PIECES EACH)",21,"TEM",1,"Simatic",1E-3,1]
["A5E02944871","SIMATIC PG, SPARE PART, ASSEMBLY HANDLE FOR FIELD PG M5/M4/M3 CONSISTING OF: 2X HANDLE, 2X HANDLE GUIDE RIGHT, 2X HANDLE GUIDE LEFT",78.800000000000011,"TEM",1,"Simatic",1E-3,1]
["A5E03306000","EVALUATION BOARD F. ERTEC 200P EB 200P, PART OF EK-ERTEC 200P INCL. POWERPLUG AND JUMPER W/O SOFTWARE W/O DOCUMENTATION",1225,"TEM",1,"Simatic",0.02,0]
["A5E03362966","SIMATIC PG, SPARE PART, SHRINK TUBING WLAN ANTENNA CABLE FOR FIELD PG M5/M4",21,"TEM",1,"Simatic",0.1,1]
["A5E03437668","SIMATIC PG, SPARE PART, BATTERY COVER FOR FIELD PG M5/M4/M3",19.5,"TEM",1,"Simatic",5.6000000000000001E-2,1]
["A5E03835763","SIMATIC PG, SPARE PART, INDICATOR BOARD FOR FIELD PG M5/M4",22.1,"TEM",1,"Simatic",0.1,1]
["A5E31210282","SIMATIC PG, SPARE PART, SATA (FLEX-) CABLE FOR FIELD PG M5/M4",18.900000000000002,"TEM",1,"Simatic",0.2,1]
["A5E31473960","SIMATIC PG, SPARE PART KIT FOAM MATERIAL(20 X A5E31315242) FOR FIELD PG M5/M4/M3",15.8,"ΠΑΚ",1,"Simatic",0.02,1]
["A5E31671633","SIMATIC PG, SPARE PART, INTERFACE COVER FOR FIELD PG M5/M4 (10 PIECES)",36.800000000000004,"TEM",1,"Simatic",0.14000000000000001,1]
["A5E33941231","IDEC BRAND LABELING LOGO! 24CE,LOGIC MODULE,DISPLAY PU/I/O: 24V/24V/24V TRANS., 8DI (4AI)/4DO; MEM 400 BLOCKS, EXPANDABLE, ETHERNET BIULD IN WEB-SERVER, DATALOG STANDARD MICRO SD CARD FOR LOGO! SOFT COMFORT V8 PREVIOS PROJECT USABEL",120,"TEM",1,"LOGO!",0.246,1]
["A5E33941234","WIDEC BRAND LABELING LOGO!230RCE,LOGIC MODULE,DISPL. PU/I/O: 115V/230V/RELAY, 8 DI/4 DO; MEM 400 BLOCKS MOD. EXPANDABLE, ETHERNET BUILT IN WEB-SERVER, DATALOG STANDARD MICRO SD CARD FOR LOGO! SOFT COMFORT V8 PREVIOUS PROJECTS EXECUTABLE",139,"TEM",1,"LOGO!",0.23899999999999999,1]
["A5E33941237","IDEC BRAND LABELING LOGO! 24RCE,LOGICMODULE,DISPLAY PU/I/O: 24V AC/24V DC/RELAY, 8 DI/4 DO; MEM. 400 BLOCKS, EXPANDABLE, ETHERNET BIULD IN WEB-SERVER, DATALOG STANDARD MICRO SD CARD FOR LOGO! SOFT COMFORT V8 PREVIOS PROJECT USABEL",136,"TEM",1,"LOGO!",0.28999999999999998,1]
["A5E33941241","IDEC BRAND LABELING LOGO!12/24RCE,LOGIC MOD.,DISPL. PU/I/O: 12/24V DC/RELAY, 8 DI (4AI)/4 DO; MEM 400 BLOCKS EXPANDABLE, ETHERNET BIULD IN WEB-SERVER, DATALOG STANDARD MICRO SD CARD FOR LOGO! SOFT COMFORT V8 PREVIOS PROJECT USABEL",136,"TEM",1,"LOGO!",0.29599999999999999,1]
["A5E33941243","IDEC BRAND LABELING LOGO! 230RCEO, LOGIC MODULE, PS/I/O: 230V/230V/RELAY, 8DI (4AI)/4DO; W/O DISPLAY, MEMORY 400 BLOCKS, EXPANDABLE MODULAR, ETHERNET BUILD IN WEB-SERVER, DATALOG, STANDARD MICRO SD CARD FOR LOGO! SOFT COMFORT V8 OR HIGHER PREVIOS PROJECTS USABLE",112,"TEM",1,"LOGO!",0.254,1]
["A5E33941244","IDEC BRAND LABELING LOGO! 24RCO (AC), LOGIC MODULE, PU/I/O: 24V AC/24V DC/RELAY, 8 DI/4 DO; W/O DISPLAY, MEMORY 400 BLOCKS, EXPANDABLE, ETHERNET BIULD IN WEB-SERVER, DATALOG STANDARD MICRO SD CARD FOR LOGO! SOFT COMFORT V8 PREVIOS PROJECT USABEL",109,"TEM",1,"LOGO!",0.254,1]
["A5E33941245","IDEC BRAND LABELING LOGO! 12/24RCEO, LOGIC MODULE PU/I/O: 12/24V DC/RELAY, 8 DI (4AI)/4 DO; W/O DISPLAY, MEMORY 400 BLOCKS EXPANDABLE, ETHERNET BIULD IN WEB-SERVER, DATALOG STANDARD MICRO SD CARD FOR LOGO! SOFT COMFORT V8 PREVIOS PROJECT USABEL",109,"TEM",1,"LOGO!",0.25,1]
["A5E33941246","IDEC BRAND LABELING LOGO! DM8 24  EXPANSION MODULE, PU/I/O: 24V/24V/TRANS., 4 DI/4 DO FOR LOGO! 8",65.100000000000009,"TEM",1,"LOGO!",0.13600000000000001,1]
["A5E33941247","IDEC BRAND LABELING LOGO! DM8 230R, EXP. MODULE, PU/I/O: 230V/230V/RELAIS, 2TE, 4 DI/4 DO FOR LOGO! 8",70.400000000000006,"TEM",1,"LOGO!",0.17199999999999999,1]
["A5E33941248","IDEC BRAND LABELING LOGO! DM8 24R EXPANSION MODULE, PU/I/O: 24V/24V/RELAY, 2TE 4 DI/4 DO,  AC/DC/NPN INPUT FOR LOGO! 8",70.400000000000006,"TEM",1,"LOGO!",0.17199999999999999,1]
["A5E33941249","IDEC BRAND LABELING LOGO! AM2  EXPANSION MODULE, PU: DC 12/24V, 2 AI, 0 - 10V OR 0/4 - 20MA FOR LOGO! 8",86.100000000000009,"TEM",1,"LOGO!",0.13700000000000001,1]
["A5E33941250","IDEC BRAND LABELING LOGO! DM8 12/24R, EXP. MODULE PU/I/O: 12, 24V/12V/24V/RELAIS, 2TE, 4 DI/4 DO FOR LOGO! 8",70.400000000000006,"TEM",1,"LOGO!",0.17199999999999999,1]
["A5E33941252","IDEC BRAND LABELING LOGO! AM2 AQ EXPAN. MODULE, PU: DC 24V, 0/4-20MA 2AQ, 0-10V FOR LOGO! 8",123,"TEM",1,"LOGO!",0.13700000000000001,1]
["A5E33941253","IDEC BRAND LABELING LOGO! TD TEXTDISPLAY, 6 LINES, 3 BACKGROUND COLORS 2 ETHERNET PORTS ACCESSORIES, FOR LOGO! 8",154,"TEM",1,"LOGO!",0.32,1]
["A5E33943265","SIMATIC PG, SPARE PART, HDD, 2,5\" 1 TB SATA FOR FIELD PG M5/M4",184,"TEM",1,"Simatic",0.25800000000000001,1]
["A5E34781577","SIMATIC PG, SPARE PART, Processor i7-3540M,up to 3.6GHz for Field PG M4",861,"TEM",1,"Simatic",0.1,1]
["A5E35678339","SIMATIC PG, spare part, flex cable ODD for Field PG M5",12.600000000000001,"TEM",1,"Simatic",0.02,1]
["A5E35697356","SIMATIC PG, spare part, motherboard for Field PG M5, with i7 processor, w/o S5 interface, w/o S5 EPrommer, w/o RAM",1890,"TEM",1,"Simatic",0.6,1]
["A5E35697378","SIMATIC PG, spare part, motherboard for Field PG M5, with i5 processor, w/o S5 interface, w/o S5 EPrommer, w/o RAM",1575,"TEM",1,"Simatic",0.6,1]
["A5E35711253","SIMATIC PG, spare part, heat sink for Field PG M5",26.3,"TEM",1,"Simatic",8.5000000000000006E-2,1]
["A5E36032292","SIMATIC PG, spare part, Wireless LAN module for Field PG M5",57.800000000000004,"TEM",1,"Simatic",0.1,1]
["A5E36285491","IDEC BRAND LABELING LOGO! SOFT COMFORT V8, SINGLE LICENSE, 1 INSTALLATION E-SW,SW AND DOCU. ON DVD, 6-LANGUAGES, EXECUTABLE UNTER WINXP, WIN7, WIN8 ALL VERISONS, 32/64 BIT MAC OSX 10.6 .. 10.9 LINUX SUSE 11.3, SP3, K 3.0.76",52.5,"TEM",1,"LOGO!",9.8000000000000004E-2,0]
["A5E36502303","SIMATIC PG, spare part, complete display housing with WLAN antennas for Field PG M5",84,"TEM",1,"Simatic",0.31,1]
["A5E36647746","SIMATIC PG, spare part, Display cable for Field PG M5",36.800000000000004,"TEM",1,"Simatic",5.0000000000000001E-3,1]
["A5E36742440","SIMATIC PG, spare part, 15,6\",  Display (16:9) Full HD for Field PG M5",289,"TEM",1,"Simatic",0.35,1]
["A5E37015313","SIMATIC PG, spare part, SSD, 2,5\" 512 GB SATA for Field PG M5",578,"TEM",1,"Simatic",0.18,1]
["A5E37015817","SIMATIC PG, spare part, SSD, 2,5\" 1 TB SATA for Field PG M5",1040,"TEM",1,"Simatic",0.2,1]
["A5E37019306","SIMATIC PG, spare part, motherboard for Field PG M5, with i7 processor, with S5 interface, with S5 EPrommer, w/o RAM",1785,"TEM",1,"Simatic",0.6,1]
["A5E37121313","SIMATIC PG, spare part, fan for Field PG M5",36.800000000000004,"TEM",1,"Simatic",0.04,1]
["A5E37745600","SIMATIC PG, spare part, slot extender Express Card for Field PG M5 5 pcs. per packaging unit",10.5,"TEM",1,"Simatic",0.06,1]
["A5E37745809","SIMATIC PG, spare part, rubber cover USB for Field PG M5 20 pcs. per packaging unit",21.6,"TEM",1,"Simatic",0.01,1]
["A5E37746165","SIMATIC PG, spare part, lower housing incl. ventilation grif for Field PG M5",147,"TEM",1,"Simatic",0.5,1]
["A5E37748116","SIMATIC PG, Spare part, keyboard module, keyboard German/International; keyboard frame, touchpad for Field PG M5",247,"TEM",1,"Simatic",0.5,1]
["A5E37748137","SIMATIC PG, Spare part, keyboard module, keyboard French; keyboard frame, touchpad for Field PG M5",247,"TEM",1,"Simatic",0.5,1]
["A5E38011975","SIMATIC PG, spare part, display parts (plaSTic), display front (5 pcs.), display buffer (20 pcs.), Siemens logo (5 pcs.) display adhesive foil (5 pcs.) for Field PG M5",52.5,"TEM",1,"Simatic",0.76500000000000001,1]
["A5E38057509","SIMATIC PG, spare part, display brake left brake, right brake for Field PG M5 5 pcs. per packaging unit",65.100000000000009,"TEM",1,"Simatic",0.245,1]
["S79220B2535E","SIMATIC IMAP V3.0 INCL. SP2 TRIAL LICENSE FOR 14 DAYS, E-SW, SW AND DOCU. ON CD, CLASS A, 5 LANGUAGES (GE/EN/FR/IT/SP), EXECUTABLE UNDER WIN7 PROF/WIN7 ULTIMATE, WINXPPROF/WINSERVER2003, REFERENCE-HW:S7-300/400, ET 200X/S, PROFINET CBA",29,"TEM",1,"Simatic",0.25,0]
["S79220B5445F888","SIMATIC STEP 7 PROF V13 ENGINEERING-SW,TRIAL365-LICENSE SW AND DOCUMENTATION ON DVD CLASS A LICENSE KEY ON USB STICK 6 LANGUAGES(GE,EN,IT,FR,SP,CH), EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64BIT), WINDOWS 8 SP1 (64 BIT), FOR CONFIGURATION OF SIMATIC S7-1200/1500 SIMATIC S7-300/400/WINAC SIMATIC BASIC PANELS",2100,"TEM",1,"Simatic",0.55400000000000005,0]
["S79220B6638F888","TIA PORTAL UPDATE COLLECTION V13 SP1 07/2015; CONTAINS 50 DVD WITH TIA PORTAL UPDATE 4, STEP 7 SAFETY UPDATE 4, WINCC RT ADVANCED UPDATE 4, WINCC RT PROFESSIONAL UPDATE 4, TIA PORTAL OPENESS UPDATE 4 AND STEP 7 PLCSIM UPDATE 1 FOR V13 SP1;",89.300000000000011,"TEM",1,"Simatic",2.5,0]
["S79220B7261F888","SIMATIC STEP 7 PROF V14 ENGINEERING-SW,TRIAL365-LICENSE SW AND DOCUMENTATION ON DVD CLASS A LICENSE KEY ON USB STICK 6 LANGUAGES(GE,EN,IT,FR,SP,CH), EXECUTABLE UNDER WINDOWS 7 (64BIT), WINDOWS 8 SP1 (64 BIT), FOR CONFIGURATION OF SIMATIC S7-1200/1500 SIMATIC S7-300/400/WINAC SIMATIC BASIC PANELS",2100,"TEM",1,"Simatic",0.44500000000000001,0]
["ZNX:100000005188","SIMATIC DP, DEVICENET HEAD ASSEMBLY FOR ET200S, CONSISTING OF: DEVICENET ADAPTER MODULE, CONNECTOR  FOR CAN, BUS TERMINATING MODULE FOR ET200S, POWER MODULE DC 24V, TERMINAL MODULE",490,"TEM",1,"Simatic",0.3,1]
["ZNX:EIP200S","SIMATIC DP, ETHERNET/IP HEAD ASSEMBLY FOR ET 200S, UP TO 63 MOUDLES INCL. MOTOR STARTERS; NO SAFTEY MODULES. INTEGRATED 2-PORT-SWITCH. CONSISTING OF: * INTERFACE MODULE INCL. TERMINATION MODULE, * SD CARD, * CONFIGURATION TOOL (DVD)",458,"TEM",1,"Simatic",0.20399999999999999,0]
["ZNX:EIP200PRO","SIMATIC DP, ETHERNET/IP HEAD ASSEMBLY FOR ET 200PRO, UP TO 12 MOUDLES INCL. MOTOR STARTERS; NO SAFTEY MODULES. INTEGRATED 2-PORT-SWITCH. INCL. CONFIGURATION TOOL (DVD)",436,"TEM",1,"Simatic",0.52800000000000002,1]
["ZNX:EIP200PROCM1","SIMATIC DP, CONNECTING MODULE FOR ETHERNET/IP HEAD ASSEMBLY ET 200PRO; M12 / 7/8\", 2 X M12 AND 2 X 7/8\",",75,"TEM",1,"Simatic",0.61699999999999999,1]
["ZNX:SYTEMA8","TANOS SYSTAINER II T-LOC ANTHRAZITE  RAL 7016",105,"TEM",1,"Simatic",1.5,0]
["6AG40121AA100XX0","SIMATIC IPC347E (RACK PC, 19\", 4U); PENTIUM DUAL CORE 3420 (2C/2T, 3.2 GHZ, 3 MB CACHE); INTERFACES: 2X GBIT ETHERNET, 1X DVI-D, 1X VGA, 2X USB FRONT, 4X USB BACK, 1X USB INTERNAL, 2X SERIAL, 2X PS/2, AUDIO; 1X 500 GBYTE HDD, INTERNAL; 2 GBYTE DDR3 SDRAM (1X 2 GBYTE), SINGLE CHANNEL; W/O OPERATING SYSTEM; 100/240 V INDUSTRIAL POWER SUPPLY, W/O POWER CORD;",982,"TEM",1,"Simatic",17,1]
["6AG40121AA210BX0","SIMATIC IPC347E (RACK PC, 19\", 4U); PENTIUM DUAL CORE 3420 (2C/2T, 3.2 GHZ, 3 MB CACHE); INTERFACES: 2X GBIT ETHERNET, 1X DVI-D, 1X VGA, 2X USB FRONT, 4X USB BACK, 1X USB INTERNAL, 2X SERIAL, 2X PS/2, AUDIO; 1X 500 GBYTE HDD, INTERNAL; 4 GBYTE DDR3 SDRAM (1X 4 GBYTE), SINGLE CHANNEL; DVD+/-RW; WINDOWS 7 ULT. 64 BIT SP1; 100/240 V INDUSTRIAL POWER SUPPLY, W/O POWER CORD;",1537,"TEM",1,"Simatic",17,1]
["6AG40121AA210XX0","SIMATIC IPC347E (RACK PC, 19\", 4U); PENTIUM DUAL CORE 3420 (2C/2T, 3.2 GHZ, 3 MB CACHE); INTERFACES: 2X GBIT ETHERNET, 1X DVI-D, 1X VGA, 2X USB FRONT, 4X USB BACK, 1X USB INTERNAL, 2X SERIAL, 2X PS/2, AUDIO; 1X 500 GBYTE HDD, INTERNAL; 4 GBYTE DDR3 SDRAM (1X 4 GBYTE), SINGLE CHANNEL; DVD+/-RW; W/O OPERATING SYSTEM; 100/240 V INDUSTRIAL POWER SUPPLY, W/O POWER CORD;",1167,"TEM",1,"Simatic",17,1]
["6AG40121CA210BX0","SIMATIC IPC347E (RACK PC, 19\", 4U); CORE I5-4570S (4C/4T, 2.9 (3.6) GHZ, 6 MB CACHE); INTERFACES: 2X GBIT ETHERNET, 1X DVI-D, 1X VGA, 2X USB FRONT, 4X USB BACK, 1X USB INTERNAL, 2X SERIAL, 2X PS/2, AUDIO; 1X 500 GBYTE HDD, INTERNAL; 4 GBYTE DDR3 SDRAM (1X 4 GBYTE), SINGLE CHANNEL; DVD+/-RW; WINDOWS 7 ULT. 64 BIT SP1; 100/240 V INDUSTRIAL POWER SUPPLY, W/O POWER CORD;",1826,"TEM",1,"Simatic",17,1]
["6AG40121CA210XX0","SIMATIC IPC347E (RACK PC, 19\", 4U); CORE I5-4570S (4C/4T, 2.9 (3.6) GHZ, 6 MB CACHE); INTERFACES: 2X GBIT ETHERNET, 1X DVI-D, 1X VGA, 2X USB FRONT, 4X USB BACK, 1X USB INTERNAL, 2X SERIAL, 2X PS/2, AUDIO; 1X 500 GBYTE HDD, INTERNAL; 4 GBYTE DDR3 SDRAM (1X 4 GBYTE), SINGLE CHANNEL; DVD+/-RW; W/O OPERATING SYSTEM; 100/240 V INDUSTRIAL POWER SUPPLY, W/O POWER CORD;",1456,"TEM",1,"Simatic",17,1]
["6AG41043CA403BX4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; PENTIUM DUAL CORE G3420 (2C/2T, 3.2 GHZ, 3 MB CACHE), 1X GBIT ETHERNET, 1X DISPLAYPORT V1.2, (IN COMBINATION WITH SHORT HOUSING ONLY); 1X 500 GB HDD, INTERNALLY MOUNTED; 16 GB DDR3 SDRAM (2X 8 GB), DUAL CHANNEL; HOUSING (SHORT) NOT PAINTED, W/O EXCHANGEABLE MEDIA; SERIAL INTERFACE (COM2) + PARALLEL (LPT); GRAPHICS ONBOARD; ADAPTER CABLE DVI-I TO VGA FOR ONBOARD GRAPHICS; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",2409,"TEM",1,"Simatic",17,1]
["6AG41043CB103XX0","SIMATIC IPC547E (RACK PC, 19\", 4U); PENTIUM DUAL CORE G3420 (2C/2T, 3.2 GHZ, 3 MB CACHE); 2X USB 3.0 FRONT, 6X USB 2.0 BACK, 1X GBIT ETHERNET, 1X DISPLAYPORT V1.2, 1X DVI-I, 2X PS/2, AUDIO; SHORT HOUSING, UNPAINTED, W/O EXCHANGEABLE MEDIA; 1X 1 TB HDD, INTERNAL; 2 GBYTE DDR3 SDRAM (1X 2 GBYTE), SINGLE CHANNEL; SERIAL (COM2) + PARALLEL (LPT), ADAPTER CABLE DVI-I TO VGA; W/O OPERATING SYSTEM; 100/240 V INDUSTRIAL POWER SUPPLY, POWER CORD EUROPE;",1559,"TEM",1,"Simatic",17,1]
["6AG41043DA220AX4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; PENTIUM DUAL CORE G3420 (2C/2T, 3.2 GHZ, 3 MB CACHE), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 1X 500 GB HDD, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2X 2 GB), DUAL CHANNEL; HOUSING NOT PAINTED, DVD+/-RW (SLIM); WITHOUT EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 32-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",2089,"TEM",1,"Simatic",17,1]
["6AG41043DA222BC4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; PENTIUM DUAL CORE G3420 (2C/2T, 3.2 GHZ, 3 MB CACHE), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 1X 500 GB HDD, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2X 2 GB), DUAL CHANNEL; HOUSING NOT PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; SIMATIC IPC DIAGMONITOR V4.5 & IMAGE&PARTITION CREATOR V3.4 ADDED; 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",2362,"TEM",1,"Simatic",17,1]
["6AG41043DA344BA4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; PENTIUM DUAL CORE G3420 (2C/2T, 3.2 GHZ, 3 MB CACHE), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 1X 500 GB HDD, INTERNALLY MOUNTED; 8 GB DDR3 SDRAM (2X 4 GB), DUAL CHANNEL; HOUSING PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT) AND PCIE X16 GRAPHICS CARD (DH:2X VGA OR 2X DVI-D); 512MB; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; SIMATIC IPC DIAGMONITOR V4,5 ADDED; 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",2761,"TEM",1,"Simatic",17,1]
["6AG41043DB243XX0","SIMATIC IPC547E (RACK PC, 19\", 4U); PENTIUM DUAL CORE G3420 (2C/2T, 3.2 GHZ, 3 MB CACHE); 2X USB 3.0 FRONT, 2X USB 3.0 & 6X USB 2.0 BACK, 1X USB 2.0 INTERNAL, 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 1X DVI-I, 1X SERIAL, 2X PS/2, AUDIO; PAINTED, DVD+/-RW (SLIM); 1X 1 TB HDD, INTERNAL; 4 GBYTE DDR3 SDRAM (2X 2 GBYTE), DUAL CHANNEL; SERIAL (COM2) + PARALLEL (LPT), ADAPTER CABLE DVI-I TO VGA; W/O OPERATING SYSTEM; 100/240 V INDUSTRIAL POWER SUPPLY, POWER CORD EUROPE;",1937,"TEM",1,"Simatic",17,1]
["6AG41043DD110BX5","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; PENTIUM DUAL CORE G3420 (2C/2T, 3.2 GHZ, 3 MB CACHE), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 2X 1 TB HDD, INTERNALLY MOUNTED; 2 GB DDR3 SDRAM (1X 2 GB), SINGLE CHANNEL; HOUSING NOT PAINTED, W/O EXCHANGEABLE MEDIA; WITHOUT EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD CHINA;",2183,"TEM",1,"Simatic",17,1]
["6AG41043DD120BX5","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; PENTIUM DUAL CORE G3420 (2C/2T, 3.2 GHZ, 3 MB CACHE), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 2X 1 TB HDD, INTERNALLY MOUNTED; 2 GB DDR3 SDRAM (1X 2 GB), SINGLE CHANNEL; HOUSING NOT PAINTED, DVD+/-RW (SLIM); WITHOUT EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD CHINA;",2267,"TEM",1,"Simatic",17,1]
["6AG41043HA220BX4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I5-4570S (4C/4T, 2.9(3.6) GHZ, 6MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 1X 500 GB HDD, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2X 2 GB), DUAL CHANNEL; HOUSING NOT PAINTED, DVD+/-RW (SLIM); WITHOUT EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",2351,"TEM",1,"Simatic",17,1]
["6AG41043HA224AX4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I5-4570S (4C/4T, 2.9(3.6) GHZ, 6MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 1X 500 GB HDD, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2X 2 GB), DUAL CHANNEL; HOUSING NOT PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT) AND PCIE X16 GRAPHICS CARD (DH:2X VGA OR 2X DVI-D); 512MB; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 32-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",2698,"TEM",1,"Simatic",17,1]
["6AG41043HA314BX0","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I5-4570S (4C/4T, 2.9(3.6) GHZ, 6MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 1X 500 GB HDD, INTERNALLY MOUNTED; 8 GB DDR3 SDRAM (2X 4 GB), DUAL CHANNEL; HOUSING NOT PAINTED, W/O EXCHANGEABLE MEDIA; SERIAL INTERFACE (COM2) + PARALLEL (LPT) AND PCIE X16 GRAPHICS CARD (DH:2X VGA OR 2X DVI-D); 512MB; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD EUROPE",2761,"TEM",1,"Simatic",17,1]
["6AG41043HD320BX4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I5-4570S (4C/4T, 2.9(3.6) GHZ, 6MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 2X 1 TB HDD, INTERNALLY MOUNTED; 8 GB DDR3 SDRAM (2X 4 GB), DUAL CHANNEL; HOUSING NOT PAINTED, DVD+/-RW (SLIM); WITHOUT EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",2761,"TEM",1,"Simatic",17,1]
["6AG41043HD342AX4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I5-4570S (4C/4T, 2.9(3.6) GHZ, 6MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 2X 1 TB HDD, INTERNALLY MOUNTED; 8 GB DDR3 SDRAM (2X 4 GB), DUAL CHANNEL; HOUSING PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 32-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",2866,"TEM",1,"Simatic",17,1]
["6AG41043HD342BX4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I5-4570S (4C/4T, 2.9(3.6) GHZ, 6MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 2X 1 TB HDD, INTERNALLY MOUNTED; 8 GB DDR3 SDRAM (2X 4 GB), DUAL CHANNEL; HOUSING PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",2866,"TEM",1,"Simatic",17,1]
["6AG41043HD342FX4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I5-4570S (4C/4T, 2.9(3.6) GHZ, 6MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 2X 1 TB HDD, INTERNALLY MOUNTED; 8 GB DDR3 SDRAM (2X 4 GB), DUAL CHANNEL; HOUSING PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT); GRAPHICS ONBOARD; WINDOWS  SERVER 2008 R2 STANDARD EDITION  INCL. 5 CLIENTS MUI (EN/GE/FR/IT/SP), 64-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",3685,"TEM",1,"Simatic",17,1]
["6AG41043HG122AX4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I5-4570S (4C/4T, 2.9(3.6) GHZ, 6MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; RAID1, 1 TB (2X 1 TB HDD, DATA MORRORING) INTERNALLY MOUNTED; 2 GB DDR3 SDRAM (1X 2 GB), SINGLE CHANNEL; HOUSING NOT PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 32-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",2687,"TEM",1,"Simatic",17,1]
["6AG41043HG322BB4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I5-4570S (4C/4T, 2.9(3.6) GHZ, 6MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; RAID1, 1 TB (2X 1 TB HDD, DATA MORRORING) INTERNALLY MOUNTED; 8 GB DDR3 SDRAM (2X 4 GB), DUAL CHANNEL; HOUSING NOT PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; SIMATIC IPC IMAGE&PARTITION CREATOR V3.4 ADDED; 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",3013,"TEM",1,"Simatic",17,1]
["6AG41043HG322FC4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I5-4570S (4C/4T, 2.9(3.6) GHZ, 6MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; RAID1, 1 TB (2X 1 TB HDD, DATA MORRORING) INTERNALLY MOUNTED; 8 GB DDR3 SDRAM (2X 4 GB), DUAL CHANNEL; HOUSING NOT PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT); GRAPHICS ONBOARD; WINDOWS  SERVER 2008 R2 STANDARD EDITION  INCL. 5 CLIENTS MUI (EN/GE/FR/IT/SP), 64-BIT, SP1; SIMATIC IPC DIAGMONITOR V4.5 & IMAGE&PARTITION CREATOR V3.4 ADDED; 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",3958,"TEM",1,"Simatic",17,1]
["6AG41043HG342AX4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I5-4570S (4C/4T, 2.9(3.6) GHZ, 6MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; RAID1, 1 TB (2X 1 TB HDD, DATA MORRORING) INTERNALLY MOUNTED; 8 GB DDR3 SDRAM (2X 4 GB), DUAL CHANNEL; HOUSING PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 32-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",2971,"TEM",1,"Simatic",17,1]
["6AG41043HP243AX0","SIMATIC IPC547E (RACK PC, 19\", 4U); CORE I5-4570S (4C/4T, 2.9 (3.6) GHZ, 6 MB CACHE, IAMT); 2X USB 3.0 FRONT, 2X USB 3.0 & 6X USB 2.0 BACK, 1X USB 2.0 INTERNAL, 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 1X DVI-I, 1X SERIAL, 2X PS/2, AUDIO; PAINTED, DVD+/-RW (SLIM); RAID1 2X 1 TBYTE IN REMOVABLE FRAME, FRONT; 4 GBYTE DDR3 SDRAM (2X 2 GBYTE), DUAL CHANNEL; SERIAL (COM2) + PARALLEL (LPT), ADAPTER CABLE DVI-I TO VGA; WINDOWS 7 ULT. 32 BIT SP1; 100/240 V INDUSTRIAL POWER SUPPLY, POWER CORD EUROPE;",3123,"TEM",1,"Simatic",17,1]
["6AG41043HP322FC4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I5-4570S (4C/4T, 2.9(3.6) GHZ, 6MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; RAID1, 1 TB (2X 1 TB HDD, DATA MORRORING) REMOVEABLE FRAME; HOT SWAP; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM (2X 4 GB), DUAL CHANNEL; HOUSING NOT PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT); GRAPHICS ONBOARD; WINDOWS  SERVER 2008 R2 STANDARD EDITION  INCL. 5 CLIENTS MUI (EN/GE/FR/IT/SP), 64-BIT, SP1; SIMATIC IPC DIAGMONITOR V4.5 & IMAGE&PARTITION CREATOR V3.4 ADDED; 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",4231,"TEM",1,"Simatic",17,1]
["6AG41043KA220AX4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 1X 500 GB HDD, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2X 2 GB), DUAL CHANNEL; HOUSING NOT PAINTED, DVD+/-RW (SLIM); WITHOUT EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 32-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",2561,"TEM",1,"Simatic",17,1]
["6AG41043KA220XX4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 1X 500 GB HDD, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2X 2 GB), DUAL CHANNEL; HOUSING NOT PAINTED, DVD+/-RW (SLIM); WITHOUT EXTENSION (HW); GRAPHICS ONBOARD; WITHOUT OPERATING SYSTEM WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",2225,"TEM",1,"Simatic",17,1]
["6AG41043KA242BC4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 1X 500 GB HDD, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2X 2 GB), DUAL CHANNEL; HOUSING PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; SIMATIC IPC DIAGMONITOR V4.5 & IMAGE&PARTITION CREATOR V3.4 ADDED; 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",2887,"TEM",1,"Simatic",17,1]
["6AG41043KA320FA4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 1X 500 GB HDD, INTERNALLY MOUNTED; 8 GB DDR3 SDRAM (2X 4 GB), DUAL CHANNEL; HOUSING NOT PAINTED, DVD+/-RW (SLIM); WITHOUT EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS  SERVER 2008 R2 STANDARD EDITION  INCL. 5 CLIENTS MUI (EN/GE/FR/IT/SP), 64-BIT, SP1; SIMATIC IPC DIAGMONITOR V4,5 ADDED; 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",3653,"TEM",1,"Simatic",17,1]
["6AG41043KA424BX4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 1X 500 GB HDD, INTERNALLY MOUNTED; 16 GB DDR3 SDRAM (2X 8 GB), DUAL CHANNEL; HOUSING NOT PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT) AND PCIE X16 GRAPHICS CARD (DH:2X VGA OR 2X DVI-D); 512MB; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",3391,"TEM",1,"Simatic",17,1]
["6AG41043KA440BA4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 1X 500 GB HDD, INTERNALLY MOUNTED; 16 GB DDR3 SDRAM (2X 8 GB), DUAL CHANNEL; HOUSING PAINTED, DVD+/-RW (SLIM); WITHOUT EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; SIMATIC IPC DIAGMONITOR V4,5 ADDED; 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",3223,"TEM",1,"Simatic",17,1]
["6AG41043KB444BA4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 1X 1 TB HDD, INTERNALLY MOUNTED; 16 GB DDR3 SDRAM (2X 8 GB), DUAL CHANNEL; HOUSING PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT) AND PCIE X16 GRAPHICS CARD (DH:2X VGA OR 2X DVI-D); 512MB; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; SIMATIC IPC DIAGMONITOR V4,5 ADDED; 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",3622,"TEM",1,"Simatic",17,1]
["6AG41043KB444BX4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 1X 1 TB HDD, INTERNALLY MOUNTED; 16 GB DDR3 SDRAM (2X 8 GB), DUAL CHANNEL; HOUSING PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT) AND PCIE X16 GRAPHICS CARD (DH:2X VGA OR 2X DVI-D); 512MB; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",3496,"TEM",1,"Simatic",17,1]
["6AG41043KD342AX4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 2X 1 TB HDD, INTERNALLY MOUNTED; 8 GB DDR3 SDRAM (2X 4 GB), DUAL CHANNEL; HOUSING PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 32-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",3076,"TEM",1,"Simatic",17,1]
["6AG41043KD342BX4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 2X 1 TB HDD, INTERNALLY MOUNTED; 8 GB DDR3 SDRAM (2X 4 GB), DUAL CHANNEL; HOUSING PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",3076,"TEM",1,"Simatic",17,1]
["6AG41043KD342FX4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 2X 1 TB HDD, INTERNALLY MOUNTED; 8 GB DDR3 SDRAM (2X 4 GB), DUAL CHANNEL; HOUSING PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT); GRAPHICS ONBOARD; WINDOWS  SERVER 2008 R2 STANDARD EDITION  INCL. 5 CLIENTS MUI (EN/GE/FR/IT/SP), 64-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",3895,"TEM",1,"Simatic",17,1]
["6AG41043KD510BX4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 2X 1 TB HDD, INTERNALLY MOUNTED; 32 GB DDR3 SDRAM (4X 8 GB), DUAL CHANNEL; HOUSING NOT PAINTED, W/O EXCHANGEABLE MEDIA; WITHOUT EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",3884,"TEM",1,"Simatic",17,1]
["6AG41043KG322BC4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; RAID1, 1 TB (2X 1 TB HDD, DATA MORRORING) INTERNALLY MOUNTED; 8 GB DDR3 SDRAM (2X 4 GB), DUAL CHANNEL; HOUSING NOT PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; SIMATIC IPC DIAGMONITOR V4.5 & IMAGE&PARTITION CREATOR V3.4 ADDED; 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",3349,"TEM",1,"Simatic",17,1]
["6AG41043KG322FC4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; RAID1, 1 TB (2X 1 TB HDD, DATA MORRORING) INTERNALLY MOUNTED; 8 GB DDR3 SDRAM (2X 4 GB), DUAL CHANNEL; HOUSING NOT PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT); GRAPHICS ONBOARD; WINDOWS  SERVER 2008 R2 STANDARD EDITION  INCL. 5 CLIENTS MUI (EN/GE/FR/IT/SP), 64-BIT, SP1; SIMATIC IPC DIAGMONITOR V4.5 & IMAGE&PARTITION CREATOR V3.4 ADDED; 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",4168,"TEM",1,"Simatic",17,1]
["6AG41043KG342AX4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; RAID1, 1 TB (2X 1 TB HDD, DATA MORRORING) INTERNALLY MOUNTED; 8 GB DDR3 SDRAM (2X 4 GB), DUAL CHANNEL; HOUSING PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 32-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",3181,"TEM",1,"Simatic",17,1]
["6AG41043KG410BA4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; RAID1, 1 TB (2X 1 TB HDD, DATA MORRORING) INTERNALLY MOUNTED; 16 GB DDR3 SDRAM (2X 8 GB), DUAL CHANNEL; HOUSING NOT PAINTED, W/O EXCHANGEABLE MEDIA; WITHOUT EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; SIMATIC IPC DIAGMONITOR V4,5 ADDED; 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",3454,"TEM",1,"Simatic",17,1]
["6AG41043KG520FX4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; RAID1, 1 TB (2X 1 TB HDD, DATA MORRORING) INTERNALLY MOUNTED; 32 GB DDR3 SDRAM (4X 8 GB), DUAL CHANNEL; HOUSING NOT PAINTED, DVD+/-RW (SLIM); WITHOUT EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS  SERVER 2008 R2 STANDARD EDITION  INCL. 5 CLIENTS MUI (EN/GE/FR/IT/SP), 64-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",4892,"TEM",1,"Simatic",17,1]
["6AG41043KM310BA6","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 2X  TB HDD REMOVABLE FRAME, FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM (2X 4 GB), DUAL CHANNEL; HOUSING NOT PAINTED, W/O EXCHANGEABLE MEDIA; WITHOUT EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; SIMATIC IPC DIAGMONITOR V4,5 ADDED; 2X 100/240V AC REDUNDANT INDUSTRIAL POWER SUPPLY; W/O POWER CORD;",3706,"TEM",1,"Simatic",17,1]
["6AG41043KM544BC6","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 2X  TB HDD REMOVABLE FRAME, FRONTSIDE MOUNTED; 32 GB DDR3 SDRAM (4X 8 GB), DUAL CHANNEL; HOUSING PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT) AND PCIE X16 GRAPHICS CARD (DH:2X VGA OR 2X DVI-D); 512MB; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; SIMATIC IPC DIAGMONITOR V4.5 & IMAGE&PARTITION CREATOR V3.4 ADDED; 2X 100/240V AC REDUNDANT INDUSTRIAL POWER SUPPLY; W/O POWER CORD;",5281,"TEM",1,"Simatic",17,1]
["6AG41043KN321BX4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; 1X 240 GB SSD REMOVABLE FRAME, FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM (2X 4 GB), DUAL CHANNEL; HOUSING NOT PAINTED, DVD+/-RW (SLIM); WITHOUT EXTENSION (HW); GRAPHICS ONBOARD; ADAPTER CABLE DVI-I TO VGA FOR ONBOARD GRAPHICS; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",3354,"TEM",1,"Simatic",17,1]
["6AG41043KP320BX4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; RAID1, 1 TB (2X 1 TB HDD, DATA MORRORING) REMOVEABLE FRAME; HOT SWAP; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM (2X 4 GB), DUAL CHANNEL; HOUSING NOT PAINTED, DVD+/-RW (SLIM); WITHOUT EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",3349,"TEM",1,"Simatic",17,1]
["6AG41043KP322BC4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; RAID1, 1 TB (2X 1 TB HDD, DATA MORRORING) REMOVEABLE FRAME; HOT SWAP; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM (2X 4 GB), DUAL CHANNEL; HOUSING NOT PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; SIMATIC IPC DIAGMONITOR V4.5 & IMAGE&PARTITION CREATOR V3.4 ADDED; 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",3622,"TEM",1,"Simatic",17,1]
["6AG41043KP341AX4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; RAID1, 1 TB (2X 1 TB HDD, DATA MORRORING) REMOVEABLE FRAME; HOT SWAP; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM (2X 4 GB), DUAL CHANNEL; HOUSING PAINTED, DVD+/-RW (SLIM); WITHOUT EXTENSION (HW); GRAPHICS ONBOARD; ADAPTER CABLE DVI-I TO VGA FOR ONBOARD GRAPHICS; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 32-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",3428,"TEM",1,"Simatic",17,1]
["6AG41043KP342FC6","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; RAID1, 1 TB (2X 1 TB HDD, DATA MORRORING) REMOVEABLE FRAME; HOT SWAP; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM (2X 4 GB), DUAL CHANNEL; HOUSING PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT); GRAPHICS ONBOARD; WINDOWS  SERVER 2008 R2 STANDARD EDITION  INCL. 5 CLIENTS MUI (EN/GE/FR/IT/SP), 64-BIT, SP1; SIMATIC IPC DIAGMONITOR V4.5 & IMAGE&PARTITION CREATOR V3.4 ADDED; 2X 100/240V AC REDUNDANT INDUSTRIAL POWER SUPPLY; W/O POWER CORD;",4913,"TEM",1,"Simatic",17,1]
["6AG41043KP344BX6","SIMATIC IPC547E (RACK PC, 19\", 4U); CORE I7-4770S (4C/8T, 3.1 (3.9) GHZ, 8 MB CACHE, IAMT); 2X USB 3.0 FRONT, 2X USB 3.0 & 6X USB 2.0 BACK, 1X USB 2.0 INTERNAL, 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 1X DVI-I, 1X SERIAL, 2X PS/2, AUDIO; PAINTED, DVD+/-RW (SLIM); RAID1 2X 1 TBYTE IN REMOVABLE FRAME, FRONT; 8 GBYTE DDR3 SDRAM (2X 4 GBYTE), DUAL CHANNEL; SERIAL (COM2) + PARALLEL (LPT), GRAPHICS CARD (DH: 2X VGA/DVI); WINDOWS 7 ULT. 64 BIT SP1; 2X 100/240 V REDUNDANT INDUSTRIAL POWER SUPPLY, W/O POWER CORD;",4168,"TEM",1,"Simatic",17,1]
["6AG41043KP420FX4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; RAID1, 1 TB (2X 1 TB HDD, DATA MORRORING) REMOVEABLE FRAME; HOT SWAP; FRONTSIDE MOUNTED; 16 GB DDR3 SDRAM (2X 8 GB), DUAL CHANNEL; HOUSING NOT PAINTED, DVD+/-RW (SLIM); WITHOUT EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS  SERVER 2008 R2 STANDARD EDITION  INCL. 5 CLIENTS MUI (EN/GE/FR/IT/SP), 64-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",4504,"TEM",1,"Simatic",17,1]
["6AG41043KP540BA4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; RAID1, 1 TB (2X 1 TB HDD, DATA MORRORING) REMOVEABLE FRAME; HOT SWAP; FRONTSIDE MOUNTED; 32 GB DDR3 SDRAM (4X 8 GB), DUAL CHANNEL; HOUSING PAINTED, DVD+/-RW (SLIM); WITHOUT EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; SIMATIC IPC DIAGMONITOR V4,5 ADDED; 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",4525,"TEM",1,"Simatic",17,1]
["6AG41043KP544BB4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; RAID1, 1 TB (2X 1 TB HDD, DATA MORRORING) REMOVEABLE FRAME; HOT SWAP; FRONTSIDE MOUNTED; 32 GB DDR3 SDRAM (4X 8 GB), DUAL CHANNEL; HOUSING PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT) AND PCIE X16 GRAPHICS CARD (DH:2X VGA OR 2X DVI-D); 512MB; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; SIMATIC IPC IMAGE&PARTITION CREATOR V3.4 ADDED; 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",4840,"TEM",1,"Simatic",17,1]
["6AG41043KQ444BX4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; RAID1, 1 TB (2X 1 TB HDD, DATA MORRORING) REMOVEABLE FRAME; HOT SWAP; FRONTSIDE MOUNTED AND 1X 1 TB HDD AS HOT SPARE IN REMOVABLE FRAME; FRONTSIDE MOUNTED: 16 GB DDR3 SDRAM (2X 8 GB), DUAL CHANNEL; HOUSING PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT) AND PCIE X16 GRAPHICS CARD (DH:2X VGA OR 2X DVI-D); 512MB; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; WITHOUT EXTENSION (SW); 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",4420,"TEM",1,"Simatic",17,1]
["6AG41043KR442BC6","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; RAID1, 1 TB (2X 1 TB HDD, DATA MORRORING) REMOVEABLE DISKS; HOT SWAP; FRONTSIDE MOUNTED AND 1X 240 GB SSD (FOR OPERTING SYSTEM) IN REMOVABLE FRAME; FRONTSIDE MOUNTED: (OPERATING SYSTEM IF ORDERED IS INSTALLED ON SSD); 16 GB DDR3 SDRAM (2X 8 GB), DUAL CHANNEL; HOUSING PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; SIMATIC IPC DIAGMONITOR V4.5 & IMAGE&PARTITION CREATOR V3.4 ADDED; 2X 100/240V AC REDUNDANT INDUSTRIAL POWER SUPPLY; W/O POWER CORD;",5176,"TEM",1,"Simatic",17,1]
["6AG41043KR510XX6","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; RAID1, 1 TB (2X 1 TB HDD, DATA MORRORING) REMOVEABLE DISKS; HOT SWAP; FRONTSIDE MOUNTED AND 1X 240 GB SSD (FOR OPERTING SYSTEM) IN REMOVABLE FRAME; FRONTSIDE MOUNTED: (OPERATING SYSTEM IF ORDERED IS INSTALLED ON SSD); 32 GB DDR3 SDRAM (4X 8 GB), DUAL CHANNEL; HOUSING NOT PAINTED, W/O EXCHANGEABLE MEDIA; WITHOUT EXTENSION (HW); GRAPHICS ONBOARD; WITHOUT OPERATING SYSTEM WITHOUT EXTENSION (SW); 2X 100/240V AC REDUNDANT INDUSTRIAL POWER SUPPLY; W/O POWER CORD;",5092,"TEM",1,"Simatic",17,1]
["6AG41043KR540BC4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; RAID1, 1 TB (2X 1 TB HDD, DATA MORRORING) REMOVEABLE DISKS; HOT SWAP; FRONTSIDE MOUNTED AND 1X 240 GB SSD (FOR OPERTING SYSTEM) IN REMOVABLE FRAME; FRONTSIDE MOUNTED: (OPERATING SYSTEM IF ORDERED IS INSTALLED ON SSD); 32 GB DDR3 SDRAM (4X 8 GB), DUAL CHANNEL; HOUSING PAINTED, DVD+/-RW (SLIM); WITHOUT EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; SIMATIC IPC DIAGMONITOR V4.5 & IMAGE&PARTITION CREATOR V3.4 ADDED; 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",5365,"TEM",1,"Simatic",17,1]
["6AG41043KT424FB0","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; RAID5, 2 TB (3X 1 TB HDD, STRIPING WITH PARITY) IN REMOVABLE FRAME; HOT SWAP; FRONTSIDE MOUNTED AND 1X 1 TB HDD AS HOT SPARE IN REMOVABLE FRAME; FRONTSIDE MOUNTED: 16 GB DDR3 SDRAM (2X 8 GB), DUAL CHANNEL; HOUSING NOT PAINTED, DVD+/-RW (SLIM); SERIAL INTERFACE (COM2) + PARALLEL (LPT) AND PCIE X16 GRAPHICS CARD (DH:2X VGA OR 2X DVI-D); 512MB; WINDOWS  SERVER 2008 R2 STANDARD EDITION  INCL. 5 CLIENTS MUI (EN/GE/FR/IT/SP), 64-BIT, SP1; SIMATIC IPC IMAGE&PARTITION CREATOR V3.4 ADDED; 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD EUROPE",5606,"TEM",1,"Simatic",17,1]
["6AG41043KT520BC4","SIMATIC IPC547E (RACK PC, 19\", 4HE); INTERFACES: 2X USB 3.0 FRONT, 1X DVI-I, 6X USB 2.0 REAR, 2X PS/2, AUDIO; 7 EXPANSION SLOTS: 2X PCIE X16, 1X PCIE X8, 4X PCI; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINERS; CORE I7-4770S (4C/8T, 3.1(3.9) GHZ, 8MB CACHE, IAMT), 2X GBIT ETHERNET, 2X DISPLAYPORT V1.2, 2X USB 3.0 REAR, 1X USB 2.0 INTERNAL, 1X COM1; RAID5, 2 TB (3X 1 TB HDD, STRIPING WITH PARITY) IN REMOVABLE FRAME; HOT SWAP; FRONTSIDE MOUNTED AND 1X 1 TB HDD AS HOT SPARE IN REMOVABLE FRAME; FRONTSIDE MOUNTED: 32 GB DDR3 SDRAM (4X 8 GB), DUAL CHANNEL; HOUSING NOT PAINTED, DVD+/-RW (SLIM); WITHOUT EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE MUI (EN/DE/FR/IT/SP), 64-BIT, SP1; SIMATIC IPC DIAGMONITOR V4.5 & IMAGE&PARTITION CREATOR V3.4 ADDED; 100/240V AC INDUSTRIAL POWER SUPPLY; POWER CORD USA;",5228,"TEM",1,"Simatic",17,1]
["6AG41044AA053XX0","SIMATIC IPC547G (RACK PC, 19\", 4U); PENTIUM DUAL CORE G4400 (2C/2T, 3.3 GHZ, 3 MB CACHE); MB (CHIPSET H110, 2X GBIT LAN, 2X USB 3.0 FRONT, 2X USB 3.0 & 4X USB 2.0 REAR, 2X PS/2, AUDIO; 1X DISPLAYPORT V1.2, 1X DVI-D, 7 SLOTS: 5x PCI-E, 2x PCI) 1X 1 TB HDD, INTERNALLY; 4 GBYTE DDR4 SDRAM (1x 4GB) HOUSING PAINTED, COM2+LPT, 100/240V AC INDUSTRIAL PS WITHOUT POWER CORD; WITHOUT OPERATING SYSTEM;",1670,"TEM",1,"Simatic",17,1]
["6AG41044GN164BX0","SIMATIC IPC547G (RACK PC, 19\", 4U); CORE i5-6500 (4C/4T, 3.2(3.6) GHz, 6MB CACHE, iAMT); MB (CHIPSET C236, 2X GBIT LAN, 2X USB3.0 FRONT, 4X USB3.0 & 4X USB2.0 REAR, 1X USB2.0 INT. 1X COM1, 2X PS/2, AUDIO; 2X DISPLAYPORT V1.2, 1X DVI-D, 7 SLOTS: 5x PCI-E, 2x PCI) RAID1 2X 1 TBYTE HDD IN REMOVABLE FRAME, FRONT; 8 GBYTE DDR4 SDRAM (2x 4GB) HOUSING PAINTED, COM2+LPT, DVD+/-RW (SLIM); ADAPTER CABLE DP NACH VGA; 100/240V AC INDUSTRIAL PS WITHOUT POWER CORD; WINDOWS 7 ULT. 64 BIT SP1;",3045,"TEM",1,"Simatic",18,1]
["6AG41044HP185BX0","SIMATIC IPC547G (RACK PC, 19\", 4U); CORE i7-6700 (4C/8T, 3.4(4.0) GHz, 8MB CACHE, iAMT); MB (CHIPSET C236, 2X GBIT LAN, 2X USB 3.0 FRONT, 4X USB 3.0 & 4X USB2.0 RUECK, 1X USB2.0 INT. 1X COM1, 2X PS/2, AUDIO; 2X DISPLAYPORT V1.2, 1X DVI-D, 7 SLOTS: 5x PCI-E, 2x PCI) RAID1 2X 1 TBYTE HDD ENTERPRISE IN REMOVABLE FRAME, FRONT; 8 GBYTE DDR4 SDRAM (2x 4GB) HOUSING PAINTED, COM2+LPT, DVD+/-RW (SLIM); GRAPHICS CARD (DH: 2X DVI/VGA); 2X 100/240 V REDUNDANT INDUSTRIAL POWER SUPPLY, WITHOUT POWER CORD; WINDOWS 7 ULT. 64 BIT SP1;",4211,"TEM",1,"Simatic",19,1]
["6AG41121GA010XX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 1 GB DDR3 SDRAM (1 X 1GB), SINGLE CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WITHOUT OPERATING SYSTEM, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",2566,"TEM",1,"Simatic",17,1]
["6AG41121GA110BX0","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 2 GB DDR3 SDRAM (1 X 2GB), SINGLE CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD EUROPE",2975,"TEM",1,"Simatic",17,1]
["6AG41121GA210QC3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1 INCLUDED; SIMATIC PC DIAGMONITOR V4.4 & IMAGE&PARTITION CREATOR  V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4298,"TEM",1,"Simatic",17,1]
["6AG41121GA214FX5","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 1 X PCI, 1 X  PCIE X8 (4 LANE), 1 X  PCIE X16, WITHOUT HW EXTENSIONS; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD CHINA",3290,"TEM",1,"Simatic",17,1]
["6AG41121GA515BB3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 2 GB DDR3 SDRAM, ECC (2 X 1GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 1 X PCI, 1 X  PCIE X8 (4 LANE), 1 X  PCIE X16; ADAPTER CABLE, DVI-I TO VGA, FOR ONBOARD GRAPHICS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, SIMATIC PC IMAGE&PARTITION CREATOR V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3159,"TEM",1,"Simatic",17,1]
["6AG41121GC212BA3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD W/O FIELDBUS; 2 X 500 GB HDD SATA; 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16 OCCUPIED; 1 X  PCIE X16 OCCUPIED; +GRAPHICS CARD PCIE X16, 256MB, (DH: 2 X DVI-D PER DP-ADAPTER); WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, SIMATIC PC DIAGMONITOR V4.4 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3868,"TEM",1,"Simatic",17,1]
["6AG41121GD010XX6","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, 0,5G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 1 GB DDR3 SDRAM (1 X 1GB), SINGLE CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WITHOUT OPERATING SYSTEM, WITHOUT SOFTWARE 2 X 110/230 IREDUNDANT POWER SUPPLY W/O POWER CORD",3301,"TEM",1,"Simatic",17,1]
["6AG41121GD213BX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, 0,5G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16 OCCUPIED; 1 X  PCIE X16 OCCUPIED; +GRAPHICS CARD PCIE X16, 256MB, (DH: 2 X VGA PER DP-ADAPTER); WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3889,"TEM",1,"Simatic",17,1]
["6AG41121GH110XX0","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, REMOVABLE DISK; FRONTSIDE MOUNTED; 2 GB DDR3 SDRAM (1 X 2GB), SINGLE CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WITHOUT OPERATING SYSTEM, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD EUROPE",2744,"TEM",1,"Simatic",17.25,1]
["6AG41121HA213EX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD  WITH PROFIBUS/MPI; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16 OCCUPIED; 1 X  PCIE X16 OCCUPIED; +GRAPHICS CARD PCIE X16, 256MB, (DH: 2 X VGA PER DP-ADAPTER); WINDOWS 7 ULTIMATE, 32BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3815,"TEM",1,"Simatic",17,1]
["6AG41121HD210BC3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD  WITH PROFIBUS/MPI; RAID1 500GB (2X 500GB HDD SATA, 0,5G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, SIMATIC PC DIAGMONITOR V4.4 & IMAGE&PARTITION CREATOR  V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3973,"TEM",1,"Simatic",17,1]
["6AG41121JA210FC3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD  WITH PROFINET (3XRJ45, CP1616 COMPATIBLE); 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; SIMATIC PC DIAGMONITOR V4.4 & IMAGE&PARTITION CREATOR  V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4088,"TEM",1,"Simatic",17,1]
["6AG41121KA010XX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 1 GB DDR3 SDRAM (1 X 1GB), SINGLE CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WITHOUT OPERATING SYSTEM, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",2702,"TEM",1,"Simatic",17,1]
["6AG41121KA080XX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 1 GB DDR3 SDRAM (1 X 1GB), SINGLE CHANNEL; WITHOUT EXCHANGEABLE MEDIA; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WITHOUT OPERATING SYSTEM, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",2545,"TEM",1,"Simatic",17,1]
["6AG41121KA110BX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 2 GB DDR3 SDRAM (1 X 2GB), SINGLE CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3112,"TEM",1,"Simatic",17,1]
["6AG41121KA210BX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3374,"TEM",1,"Simatic",17,1]
["6AG41121KA214PX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 1 X PCI, 1 X  PCIE X8 (4 LANE), 1 X  PCIE X16, WITHOUT HW EXTENSIONS; WINDOWS SERVER 2008 STANDARD EDITION INCL. 5 CLIENT, 32BIT, MUI (EN, GE, FR, IT, SP),SP2; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4246,"TEM",1,"Simatic",17,1]
["6AG41121KA284PA3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; WITHOUT EXCHANGEABLE MEDIA; BOARD WITH 3 SLOTS: 1 X PCI, 1 X  PCIE X8 (4 LANE), 1 X  PCIE X16, WITHOUT HW EXTENSIONS; WINDOWS SERVER 2008 STANDARD EDITION INCL. 5 CLIENT, 32BIT, MUI (EN, GE, FR, IT, SP),SP2; SIMATIC PC DIAGMONITOR V4.4 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4214,"TEM",1,"Simatic",17,1]
["6AG41121KA310FX6","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 6 GB DDR3 SDRAM (1X2GB, 1X4GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 2 X 110/230 IREDUNDANT POWER SUPPLY W/O POWER CORD",4088,"TEM",1,"Simatic",17,1]
["6AG41121KA410FX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 8 GB DDR3 SDRAM (2 X 4GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3931,"TEM",1,"Simatic",17,1]
["6AG41121KA412FX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 8 GB DDR3 SDRAM (2 X 4GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16 OCCUPIED; 1 X  PCIE X16 OCCUPIED; +GRAPHICS CARD PCIE X16, 256MB, (DH: 2 X DVI-D PER DP-ADAPTER); WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4225,"TEM",1,"Simatic",17,1]
["6AG41121KA413FX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 8 GB DDR3 SDRAM (2 X 4GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16 OCCUPIED; 1 X  PCIE X16 OCCUPIED; +GRAPHICS CARD PCIE X16, 256MB, (DH: 2 X VGA PER DP-ADAPTER); WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4267,"TEM",1,"Simatic",17,1]
["6AG41121KA610FX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM, ECC (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3511,"TEM",1,"Simatic",17,1]
["6AG41121KB210PX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 500 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS SERVER 2008 STANDARD EDITION INCL. 5 CLIENT, 32BIT, MUI (EN, GE, FR, IT, SP),SP2; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4277,"TEM",1,"Simatic",17,1]
["6AG41121KD380BX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, 0,5G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 6 GB DDR3 SDRAM (1X2GB, 1X4GB), DUAL CHANNEL; WITHOUT EXCHANGEABLE MEDIA; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3794,"TEM",1,"Simatic",17,1]
["6AG41121KD680BA0","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, 0,5G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM, ECC (2 X 2GB), DUAL CHANNEL; WITHOUT EXCHANGEABLE MEDIA; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, SIMATIC PC DIAGMONITOR V4.4 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD EUROPE",3763,"TEM",1,"Simatic",17,1]
["6AG41121KD680BA3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, 0,5G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM, ECC (2 X 2GB), DUAL CHANNEL; WITHOUT EXCHANGEABLE MEDIA; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, SIMATIC PC DIAGMONITOR V4.4 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3763,"TEM",1,"Simatic",17,1]
["6AG41121KK210BX6","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 500 GB HDD SATA, REMOVABLE DISK; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 2 X 110/230 IREDUNDANT POWER SUPPLY W/O POWER CORD",3920,"TEM",1,"Simatic",17.25,1]
["6AG41121KP210BA3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, SIMATIC PC DIAGMONITOR V4.4 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4004,"TEM",1,"Simatic",17.25,1]
["6AG41121KP210XA3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WITHOUT OPERATING SYSTEM, SIMATIC PC DIAGMONITOR V4.4 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3700,"TEM",1,"Simatic",17.25,1]
["6AG41121KP211XA0","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; ADAPTER CABLE, DVI-I TO VGA, FOR ONBOARD GRAPHICS; WITHOUT OPERATING SYSTEM, SIMATIC PC DIAGMONITOR V4.4 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD EUROPE",3726,"TEM",1,"Simatic",17.25,1]
["6AG41121KP212EX0","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16 OCCUPIED; 1 X  PCIE X16 OCCUPIED; +GRAPHICS CARD PCIE X16, 256MB, (DH: 2 X DVI-D PER DP-ADAPTER); WINDOWS 7 ULTIMATE, 32BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD EUROPE",4204,"TEM",1,"Simatic",17.25,1]
["6AG41121KP610BX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM, ECC (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3983,"TEM",1,"Simatic",17.25,1]
["6AG41121KP611EX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM, ECC (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; ADAPTER CABLE, DVI-I TO VGA, FOR ONBOARD GRAPHICS; WINDOWS 7 ULTIMATE, 32BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4041,"TEM",1,"Simatic",17.25,1]
["6AG41121KS610FX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 50 GB SSD (SLC) SATA; INTERNALLY MOUNTED; 4 GB DDR3 SDRAM, ECC (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3983,"TEM",1,"Simatic",17,1]
["6AG41121LA181EX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD WITH PROFIBUS/MPI; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 2 GB DDR3 SDRAM (1 X 2GB), SINGLE CHANNEL; WITHOUT EXCHANGEABLE MEDIA; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; ADAPTER CABLE, DVI-I TO VGA, FOR ONBOARD GRAPHICS; WINDOWS 7 ULTIMATE, 32BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3222,"TEM",1,"Simatic",17,1]
["6AG41121LP211BC3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD WITH PROFIBUS/MPI; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; ADAPTER CABLE, DVI-I TO VGA, FOR ONBOARD GRAPHICS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, SIMATIC PC DIAGMONITOR V4.4 & IMAGE&PARTITION CREATOR  V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4324,"TEM",1,"Simatic",17.25,1]
["6AG41121NA211BX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; ADAPTER CABLE, DVI-I TO VGA, FOR ONBOARD GRAPHICS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3589,"TEM",1,"Simatic",17,1]
["6AG41121NA214BX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 1 X PCI, 1 X  PCIE X8 (4 LANE), 1 X  PCIE X16, WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3584,"TEM",1,"Simatic",17,1]
["6AG41121NA410FA6","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 8 GB DDR3 SDRAM (2 X 4GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; SIMATIC PC DIAGMONITOR V4.4 INCLUDED; 2 X 110/230 IREDUNDANT POWER SUPPLY W/O POWER CORD",4666,"TEM",1,"Simatic",17,1]
["6AG41121NB210QX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 500 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4466,"TEM",1,"Simatic",17,1]
["6AG41121NB284FX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 500 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; WITHOUT EXCHANGEABLE MEDIA; BOARD WITH 3 SLOTS: 1 X PCI, 1 X  PCIE X8 (4 LANE), 1 X  PCIE X16, WITHOUT HW EXTENSIONS; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3511,"TEM",1,"Simatic",17,1]
["6AG41121ND410FX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, 0,5G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 8 GB DDR3 SDRAM (2 X 4GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4435,"TEM",1,"Simatic",17,1]
["6AG41121ND710QX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, 0,5G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 8 GB DDR3 SDRAM, ECC (2 X 4GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",5464,"TEM",1,"Simatic",17,1]
["6AG41121NH214XX6","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, REMOVABLE DISK; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 1 X PCI, 1 X  PCIE X8 (4 LANE), 1 X  PCIE X16, WITHOUT HW EXTENSIONS; WITHOUT OPERATING SYSTEM, WITHOUT SOFTWARE 2 X 110/230 IREDUNDANT POWER SUPPLY W/O POWER CORD",3773,"TEM",1,"Simatic",17.25,1]
["6AG41121NM214XX6","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 2 X 500 GB HDD SATA; REMOVABLE DISK; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 1 X PCI, 1 X  PCIE X8 (4 LANE), 1 X  PCIE X16, WITHOUT HW EXTENSIONS; WITHOUT OPERATING SYSTEM, WITHOUT SOFTWARE 2 X 110/230 IREDUNDANT POWER SUPPLY W/O POWER CORD",4099,"TEM",1,"Simatic",17,1]
["6AG41121NP211PX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; ADAPTER CABLE, DVI-I TO VGA, FOR ONBOARD GRAPHICS; WINDOWS SERVER 2008 STANDARD EDITION INCL. 5 CLIENT, 32BIT, MUI (EN, GE, FR, IT, SP),SP2; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4944,"TEM",1,"Simatic",17.25,1]
["6AG41121NP212XC6","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16 OCCUPIED; 1 X  PCIE X16 OCCUPIED; +GRAPHICS CARD PCIE X16, 256MB, (DH: 2 X DVI-D PER DP-ADAPTER); WITHOUT OPERATING SYSTEM, SIMATIC PC DIAGMONITOR V4.4 & IMAGE&PARTITION CREATOR  V3.3 INCLUDED; 2 X 110/230 IREDUNDANT POWER SUPPLY W/O POWER CORD",4687,"TEM",1,"Simatic",17.25,1]
["6AG41121NP216PX0","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 1 X PCI, 1 X  PCIE X8 (4 LANE), 1 X  PCIE X16 OCCUPIED; +GRAPHICS CARD PCIE X16, 256MB, (DH: 2 X DVI-D PER DP-ADAPTER); WINDOWS SERVER 2008 STANDARD EDITION INCL. 5 CLIENT, 32BIT, MUI (EN, GE, FR, IT, SP),SP2; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD EUROPE",5233,"TEM",1,"Simatic",17.25,1]
["6AG41121NP611FX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM, ECC (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; ADAPTER CABLE, DVI-I TO VGA, FOR ONBOARD GRAPHICS; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4230,"TEM",1,"Simatic",17.25,1]
["6AG41121NP615BB3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM, ECC (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 1 X PCI, 1 X  PCIE X8 (4 LANE), 1 X  PCIE X16; ADAPTER CABLE, DVI-I TO VGA, FOR ONBOARD GRAPHICS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, SIMATIC PC IMAGE&PARTITION CREATOR V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4303,"TEM",1,"Simatic",17.25,1]
["6AG41121NP615QB3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM, ECC (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 1 X PCI, 1 X  PCIE X8 (4 LANE), 1 X  PCIE X16; ADAPTER CABLE, DVI-I TO VGA, FOR ONBOARD GRAPHICS; WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1 INCLUDED; SIMATIC PC IMAGE&PARTITION CREATOR V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",5154,"TEM",1,"Simatic",17.25,1]
["6AG41121NP616XC3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM, ECC (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 1 X PCI, 1 X  PCIE X8 (4 LANE), 1 X  PCIE X16 OCCUPIED; +GRAPHICS CARD PCIE X16, 256MB, (DH: 2 X DVI-D PER DP-ADAPTER); WITHOUT OPERATING SYSTEM, SIMATIC PC DIAGMONITOR V4.4 & IMAGE&PARTITION CREATOR  V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4393,"TEM",1,"Simatic",17.25,1]
["6AG41121NP714QA6","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM, ECC (2 X 4GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 1 X PCI, 1 X  PCIE X8 (4 LANE), 1 X  PCIE X16, WITHOUT HW EXTENSIONS; WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1 INCLUDED; SIMATIC PC DIAGMONITOR V4.4 INCLUDED; 2 X 110/230 IREDUNDANT POWER SUPPLY W/O POWER CORD",6220,"TEM",1,"Simatic",17.25,1]
["6AG41121NP715QB3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM, ECC (2 X 4GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 1 X PCI, 1 X  PCIE X8 (4 LANE), 1 X  PCIE X16; ADAPTER CABLE, DVI-I TO VGA, FOR ONBOARD GRAPHICS; WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1 INCLUDED; SIMATIC PC IMAGE&PARTITION CREATOR V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",5784,"TEM",1,"Simatic",17.25,1]
["6AG41121NS710QX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 50 GB SSD (SLC) SATA; INTERNALLY MOUNTED; 8 GB DDR3 SDRAM, ECC (2 X 4GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",5621,"TEM",1,"Simatic",17,1]
["6AG41121NT214XX6","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 50 GB SSD (SLC) SATA; REMOVABLE DISK; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 1 X PCI, 1 X  PCIE X8 (4 LANE), 1 X  PCIE X16, WITHOUT HW EXTENSIONS; WITHOUT OPERATING SYSTEM, WITHOUT SOFTWARE 2 X 110/230 IREDUNDANT POWER SUPPLY W/O POWER CORD",4288,"TEM",1,"Simatic",17,1]
["6AG41121PD214EX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD WITH PROFIBUS/MPI; RAID1 500GB (2X 500GB HDD SATA, 0,5G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 1 X PCI, 1 X  PCIE X8 (4 LANE), 1 X  PCIE X16, WITHOUT HW EXTENSIONS; WINDOWS 7 ULTIMATE, 32BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4141,"TEM",1,"Simatic",17,1]
["6AG41121PM213EX3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD WITH PROFIBUS/MPI; 2 X 500 GB HDD SATA; REMOVABLE DISK; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16 OCCUPIED; 1 X  PCIE X16 OCCUPIED; +GRAPHICS CARD PCIE X16, 256MB, (DH: 2 X VGA PER DP-ADAPTER); WINDOWS 7 ULTIMATE, 32BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4540,"TEM",1,"Simatic",17,1]
["6AG41121PP615BB3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD WITH PROFIBUS/MPI; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM, ECC (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 1 X PCI, 1 X  PCIE X8 (4 LANE), 1 X  PCIE X16; ADAPTER CABLE, DVI-I TO VGA, FOR ONBOARD GRAPHICS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, SIMATIC PC IMAGE&PARTITION CREATOR V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4513,"TEM",1,"Simatic",17.25,1]
["6AG41121PP616XC3","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD WITH PROFIBUS/MPI; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM, ECC (2 X 2GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 1 X PCI, 1 X  PCIE X8 (4 LANE), 1 X  PCIE X16 OCCUPIED; +GRAPHICS CARD PCIE X16, 256MB, (DH: 2 X DVI-D PER DP-ADAPTER); WITHOUT OPERATING SYSTEM, SIMATIC PC DIAGMONITOR V4.4 & IMAGE&PARTITION CREATOR  V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4603,"TEM",1,"Simatic",17.25,1]
["6AG41121PU711FA6","SIMATIC IPC647C (RACK PC, 19\", 2U); INTERFACES:2 X GBIT LAN (RJ45), 1 X DVI-I; AUDIO, 2 X COM; 1 X LPT; 2 X PS/2; 4X USB 2.0 BACKSIDE, 2X USB 2.0 FRONTSIDE; 1X USB 2.0  INTERNALLY; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD WITH PROFIBUS/MPI; RAID1 1TB (2 X 1 TB HDD SAS), REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; PCIE X8 RAID CONTROLLER IN PCIE X16 SLOT; 8 GB DDR3 SDRAM, ECC (2 X 4GB), DUAL CHANNEL; DVD +/- RW, SLIMLINE; BOARD WITH 3 SLOTS: 2 X PCI, 1 X  PCIE X16; ADAPTER CABLE, DVI-I TO VGA, FOR ONBOARD GRAPHICS; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; SIMATIC PC DIAGMONITOR V4.4 INCLUDED; 2 X 110/230 IREDUNDANT POWER SUPPLY W/O POWER CORD",7138,"TEM",1,"Simatic",17.25,1]
["6AG41122DA300BX3","SIMATIC IPC647D (RACK PC, 19\", 2U); 2X GBIT ETHERNET(IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0, INKL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I3-4330TE (2C/4T, 2.4GHZ, 4MB CACHE); MAINBOARD W/O FIELDBUS; 500 GB HDD SATA, INTERNALLY MOUNTED; (0,5 G VIBRATION, 5 G SHOCK); 8 GB DDR3 SDRAM (2X 4GB), DUAL CHANNEL; BOARD WITH 2 SLOTS: 2X PCIE X16; WITHOUT HW EXTENSIONS; W/O EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; WITHOUT EXTENSION (SW); 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD USA",2699,"TEM",1,"Simatic",14,1]
["6AG41122DS231BX3","SIMATIC IPC647D (RACK PC, 19\", 2U); 2X GBIT ETHERNET(IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0, INKL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I3-4330TE (2C/4T, 2.4GHZ, 4MB CACHE); MAINBOARD W/O FIELDBUS; 240 GB SSD SATA, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2X 2GB), DUAL CHANNEL; BOARD WITH 2 SLOTS: 2X PCIE X16; DVD +/- RW (SLIM); W/O EXTENSION (HW); GRAPHICS ONBOARD; ADAPTER CABLE DVI-I TO VGA FOR ONBOARD GRAPHICS; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; WITHOUT EXTENSION (SW); 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD USA",3187,"TEM",1,"Simatic",14,1]
["6AG41122GA350BC3","SIMATIC IPC647D (RACK PC, 19\", 2U); 2X GBIT ETHERNET(IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0, INKL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-4570TE (2C/4T, 2.7(3.3) GHZ, 4MB CACHE, TB,VT-D, AMT); MAINBOARD W/O FELDBUS; 500 GB HDD SATA, INTERNALLY MOUNTED; (0,5 G VIBRATION, 5 G SHOCK); 8 GB DDR3 SDRAM (2X 4GB), DUAL CHANNEL; BOARD WITH 4 SLOTS: 4X PCIE X16; DVD +/- RW (SLIM); W/O EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; SIMATIC PC DIAGMONITOR V4.5 AND IMAGE&PARTITION CREATOR  V3.4 INCLUDED; 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD USA",3297,"TEM",1,"Simatic",14,1]
["6AG41122GA350BX3","SIMATIC IPC647D (RACK PC, 19\", 2U); 2X GBIT ETHERNET(IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0, INKL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-4570TE (2C/4T, 2.7(3.3) GHZ, 4MB CACHE, TB,VT-D, AMT); MAINBOARD W/O FELDBUS; 500 GB HDD SATA, INTERNALLY MOUNTED; (0,5 G VIBRATION, 5 G SHOCK); 8 GB DDR3 SDRAM (2X 4GB), DUAL CHANNEL; BOARD WITH 4 SLOTS: 4X PCIE X16; DVD +/- RW (SLIM); W/O EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; WITHOUT EXTENSION (SW); 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD USA",3077,"TEM",1,"Simatic",14,1]
["6AG41122GB434FA3","SIMATIC IPC647D (RACK PC, 19\", 2U); 2X GBIT ETHERNET(IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0, INKL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-4570TE (2C/4T, 2.7(3.3) GHZ, 4MB CACHE, TB,VT-D, AMT); MAINBOARD W/O FELDBUS; 1 TB HDD SATA, INTERNALLY MOUNTED; (0,5 G VIBRATION, 5 G SHOCK); 16 GB DDR3 SDRAM (2X 8GB), DUAL CHANNEL; BOARD WITH 2 SLOTS: 2X PCIE X16; DVD +/- RW (SLIM); COM2; LPT (1 SLOT OCCUPIED); +PCIE X16 GRAPHICS CARD (DUAL HEAD: 2X VGA OR 2X DVI-D), 512MB, (1 SLOT OCCUPIED); WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; SIMATIC PC DIAGMONITOR V4.5 INCLUDED; 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD USA",4662,"TEM",1,"Simatic",14,1]
["6AG41122GP240BX6","SIMATIC IPC647D (RACK PC, 19\", 2U); 2X GBIT ETHERNET(IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0, INKL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-4570TE (2C/4T, 2.7(3.3) GHZ, 4MB CACHE, TB,VT-D, AMT); MAINBOARD W/O FELDBUS; RAID1, 1 TB (2X 1 TB HDD SATA, DATA MIRRORING), REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2X 2GB), DUAL CHANNEL; BOARD WITH 4 SLOTS: 2X PCI, 2X PCIE X16; DVD +/- RW (SLIM); W/O EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; WITHOUT EXTENSION (SW); 2 X 110/240V REDUNDANT POWER SUPPLY W/O POWER CORD",3833,"TEM",1,"Simatic",14,1]
["6AG41122GT240BX6","SIMATIC IPC647D (RACK PC, 19\", 2U); 2X GBIT ETHERNET(IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0, INKL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; CORE I5-4570TE (2C/4T, 2.7(3.3) GHZ, 4MB CACHE, TB,VT-D, AMT); MAINBOARD W/O FELDBUS; 240 GB SSD SATA, REMOVABLE DISK; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2X 2GB), DUAL CHANNEL; BOARD WITH 4 SLOTS: 2X PCI, 2X PCIE X16; DVD +/- RW (SLIM); W/O EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; WITHOUT EXTENSION (SW); 2 X 110/240V REDUNDANT POWER SUPPLY W/O POWER CORD",3917,"TEM",1,"Simatic",14.25,1]
["6AG41122KA610BC3","SIMATIC IPC647D (RACK PC, 19\", 2U); 2X GBIT ETHERNET(IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0, INKL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; XEON E3-1268LV3 (4C/8T, 2.3(3.3) GHZ, 8MB CACHE VT-D, AMT); MAINBOARD W/O FELDBUS; 500 GB HDD SATA, INTERNALLY MOUNTED; (0,5 G VIBRATION, 5 G SHOCK); 8 GB DDR3 SDRAM (2X 4GB), ECC, DUAL CHANNEL; BOARD WITH 4 SLOTS: 2X PCI, 2X PCIE X16; WITHOUT HW EXTENSIONS; W/O EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; SIMATIC PC DIAGMONITOR V4.5 AND IMAGE&PARTITION CREATOR  V3.4 INCLUDED; 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD USA",3612,"TEM",1,"Simatic",14,1]
["6AG41122KD711FX3","SIMATIC IPC647D (RACK PC, 19\", 2U); 2X GBIT ETHERNET(IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0, INKL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; XEON E3-1268LV3 (4C/8T, 2.3(3.3) GHZ, 8MB CACHE VT-D, AMT); MAINBOARD W/O FELDBUS; RAID1, 1 TB (2X 1 TB HDD SATA, DATA MIRRORING), INTERNALLY MOUNTED; 0,5G VIBRATION, 5 G SHOCK, 16 GB DDR3 SDRAM (2X 8GB), ECC, DUAL CHANNEL; BOARD WITH 4 SLOTS: 2X PCI, 2X PCIE X16; WITHOUT HW EXTENSIONS; W/O EXTENSION (HW); GRAPHICS ONBOARD; ADAPTER CABLE DVI-I TO VGA FOR ONBOARD GRAPHICS; WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; WITHOUT EXTENSION (SW); 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD USA",5046,"TEM",1,"Simatic",14,1]
["6AG41122KP431FX3","SIMATIC IPC647D (RACK PC, 19\", 2U); 2X GBIT ETHERNET(IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0, INKL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; XEON E3-1268LV3 (4C/8T, 2.3(3.3) GHZ, 8MB CACHE VT-D, AMT); MAINBOARD W/O FELDBUS; RAID1, 1 TB (2X 1 TB HDD SATA, DATA MIRRORING), REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 16 GB DDR3 SDRAM (2X 8GB), DUAL CHANNEL; BOARD WITH 2 SLOTS: 2X PCIE X16; DVD +/- RW (SLIM); W/O EXTENSION (HW); GRAPHICS ONBOARD; ADAPTER CABLE DVI-I TO VGA FOR ONBOARD GRAPHICS; WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; WITHOUT EXTENSION (SW); 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD USA",4951,"TEM",1,"Simatic",14,1]
["6AG41122KP432FC3","SIMATIC IPC647D (RACK PC, 19\", 2U); 2X GBIT ETHERNET(IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0, INKL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; XEON E3-1268LV3 (4C/8T, 2.3(3.3) GHZ, 8MB CACHE VT-D, AMT); MAINBOARD W/O FELDBUS; RAID1, 1 TB (2X 1 TB HDD SATA, DATA MIRRORING), REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 16 GB DDR3 SDRAM (2X 8GB), DUAL CHANNEL; BOARD WITH 2 SLOTS: 2X PCIE X16; DVD +/- RW (SLIM); COM2; LPT (1 SLOT OCCUPIED); GRAPHICS ONBOARD; WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; SIMATIC PC DIAGMONITOR V4.5 AND IMAGE&PARTITION CREATOR  V3.4 INCLUDED; 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD USA",5208,"TEM",1,"Simatic",14,1]
["6AG41122KP531FX3","SIMATIC IPC647D (RACK PC, 19\", 2U); 2X GBIT ETHERNET(IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0, INKL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; XEON E3-1268LV3 (4C/8T, 2.3(3.3) GHZ, 8MB CACHE VT-D, AMT); MAINBOARD W/O FELDBUS; RAID1, 1 TB (2X 1 TB HDD SATA, DATA MIRRORING), REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 32 GB DDR3 SDRAM (4X 8GB), DUAL CHANNEL; BOARD WITH 2 SLOTS: 2X PCIE X16; DVD +/- RW (SLIM); W/O EXTENSION (HW); GRAPHICS ONBOARD; ADAPTER CABLE DVI-I TO VGA FOR ONBOARD GRAPHICS; WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; WITHOUT EXTENSION (SW); 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD USA",5613,"TEM",1,"Simatic",14,1]
["6AG41122KT743FC3","SIMATIC IPC647D (RACK PC, 19\", 2U); 2X GBIT ETHERNET(IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0, INKL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; XEON E3-1268LV3 (4C/8T, 2.3(3.3) GHZ, 8MB CACHE VT-D, AMT); MAINBOARD W/O FELDBUS; 240 GB SSD SATA, REMOVABLE DISK; FRONTSIDE MOUNTED; 16 GB DDR3 SDRAM (2X 8GB), ECC, DUAL CHANNEL; BOARD WITH 4 SLOTS: 2X PCI, 2X PCIE X16; DVD +/- RW (SLIM); COM2; LPT (1 SLOT OCCUPIED); GRAPHICS ONBOARD; ADAPTER CABLE DVI-I TO VGA FOR ONBOARD GRAPHICS; WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; SIMATIC PC DIAGMONITOR V4.5 AND IMAGE&PARTITION CREATOR  V3.4 INCLUDED; 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD USA",5739,"TEM",1,"Simatic",14.25,1]
["6AG41122MH800BC3","SIMATIC IPC647D (RACK PC, 19\", 2U); 2X GBIT ETHERNET(IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0, INKL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; XEON E3-1268LV3 (4C/8T, 2.3(3.3) GHZ, 8MB CACHE VT-D, AMT); MAINBOARD WITH PROFINET (3X RJ45, CP1616-COMPATIBLE); 500 GB HDD SATA, REMOVABLE DISK; FRONTSIDE MOUNTED; 32 GB DDR3 SDRAM (4X 8GB), ECC, DUAL CHANNEL; BOARD WITH 2 SLOTS: 2X PCIE X16; WITHOUT HW EXTENSIONS; W/O EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; SIMATIC PC DIAGMONITOR V4.5 AND IMAGE&PARTITION CREATOR  V3.4 INCLUDED; 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD USA",5712,"TEM",1,"Simatic",14.25,1]
["6AG41122MT642AA0","SIMATIC IPC647D (RACK PC, 19\", 2U); 2X GBIT ETHERNET(IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0, INKL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER; XEON E3-1268LV3 (4C/8T, 2.3(3.3) GHZ, 8MB CACHE VT-D, AMT); MAINBOARD WITH PROFINET (3X RJ45, CP1616-COMPATIBLE); 240 GB SSD SATA, REMOVABLE DISK; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM (2X 4GB), ECC, DUAL CHANNEL; BOARD WITH 4 SLOTS: 2X PCI, 2X PCIE X16; DVD +/- RW (SLIM); COM2; LPT (1 SLOT OCCUPIED); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE, 32BIT, MUI (EN, GE, FR, IT, SP), SP1; SIMATIC PC DIAGMONITOR V4.5 INCLUDED; 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD EUROPE",4914,"TEM",1,"Simatic",14.25,1]
["6AG41141GA014XX0","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 1 GB DDR3 SDRAM (1 X 1GB), SINGLE CHANNEL; DVD-ROM; BOARD WITH 11 SLOTS: 7 X PCI, 1 X  PCIE X16, 3 X PCIE X4; WITHOUT HW EXTENSIONS; WITHOUT OPERATING SYSTEM, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD EUROPE",2650,"TEM",1,"Simatic",17,1]
["6AG41141GA120BX0","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 2 GB DDR3 SDRAM (1 X 2GB), SINGLE CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD EUROPE",3007,"TEM",1,"Simatic",17,1]
["6AG41141GA120BX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 2 GB DDR3 SDRAM (1 X 2GB), SINGLE CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3007,"TEM",1,"Simatic",17,1]
["6AG41141GA120EX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 2 GB DDR3 SDRAM (1 X 2GB), SINGLE CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS 7 ULTIMATE, 32BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3038,"TEM",1,"Simatic",17,1]
["6AG41141GA220EX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS 7 ULTIMATE, 32BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3301,"TEM",1,"Simatic",17,1]
["6AG41141GA221NX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; DVI-VGA-ADAPTER FOR ONBOARD GRAPHICS; WINDOWS SERVER 2003 R2 STANDARD EDITION INCL. 5 CLIENT, 32BIT, MUI (EN, GE, FR, IT, SP),SP2; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4146,"TEM",1,"Simatic",17,1]
["6AG41141GB210EX0","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD W/O FIELDBUS; 500 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD-ROM; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS 7 ULTIMATE, 32BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD EUROPE",3269,"TEM",1,"Simatic",17,1]
["6AG41141GD010BX2","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, 0,5G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 1 GB DDR3 SDRAM (1 X 1GB), SINGLE CHANNEL; DVD-ROM; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD SWITZERLAND",3133,"TEM",1,"Simatic",17,1]
["6AG41141GG120BX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA; 0,3 G VIBRATION, 3 G SHOCK, INTERNALLY MOUNTED; 2 GB DDR3 SDRAM (1 X 2GB), SINGLE CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",2954,"TEM",1,"Simatic",17,1]
["6AG41141GG221EX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA; 0,3 G VIBRATION, 3 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; DVI-VGA-ADAPTER FOR ONBOARD GRAPHICS; WINDOWS 7 ULTIMATE, 32BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3274,"TEM",1,"Simatic",17,1]
["6AG41141GH020BA0","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, REMOVABLE DISK; FRONTSIDE MOUNTED; 1 GB DDR3 SDRAM (1 X 1GB), SINGLE CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, SIMATIC PC DIAGMONITOR V4.4 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD EUROPE",3101,"TEM",1,"Simatic",17.25,1]
["6AG41141GH110BX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, REMOVABLE DISK; FRONTSIDE MOUNTED; 2 GB DDR3 SDRAM (1 X 2GB), SINGLE CHANNEL; DVD-ROM; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",2996,"TEM",1,"Simatic",17.25,1]
["6AG41141GM111BC3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD W/O FIELDBUS; 2 X 500 GB HDD SATA; REMOVABLE DISK; FRONTSIDE MOUNTED; 2 GB DDR3 SDRAM (1 X 2GB), SINGLE CHANNEL; DVD-ROM; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; DVI-VGA-ADAPTER FOR ONBOARD GRAPHICS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, SIMATIC PC DIAGMONITOR V4.4 & IMAGE&PARTITION CREATOR  V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3568,"TEM",1,"Simatic",17,1]
["6AG41141GP020BX0","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 1 GB DDR3 SDRAM (1 X 1GB), SINGLE CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD EUROPE",3416,"TEM",1,"Simatic",17.25,1]
["6AG41141GP121BX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 2 GB DDR3 SDRAM (1 X 2GB), SINGLE CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; DVI-VGA-ADAPTER FOR ONBOARD GRAPHICS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3547,"TEM",1,"Simatic",17.25,1]
["6AG41141HC220BA0","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD  WITH PROFIBUS/MPI; 2 X 500 GB HDD SATA; 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, SIMATIC PC DIAGMONITOR V4.4 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD EUROPE",3815,"TEM",1,"Simatic",17,1]
["6AG41141HG080BX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD  WITH PROFIBUS/MPI; 250 GB HDD SATA; 0,3 G VIBRATION, 3 G SHOCK, INTERNALLY MOUNTED; 1 GB DDR3 SDRAM (1 X 1GB), SINGLE CHANNEL; WITHOUT EXCHANGEABLE MEDIA; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",2923,"TEM",1,"Simatic",17,1]
["6AG41141HG084BX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD  WITH PROFIBUS/MPI; 250 GB HDD SATA; 0,3 G VIBRATION, 3 G SHOCK, INTERNALLY MOUNTED; 1 GB DDR3 SDRAM (1 X 1GB), SINGLE CHANNEL; WITHOUT EXCHANGEABLE MEDIA; BOARD WITH 11 SLOTS: 7 X PCI, 1 X  PCIE X16, 3 X PCIE X4; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3059,"TEM",1,"Simatic",17,1]
["6AG41141HS211BB3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD  WITH PROFIBUS/MPI; 50 GB SSD SATA; INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD-ROM; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; DVI-VGA-ADAPTER FOR ONBOARD GRAPHICS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, SIMATIC PC IMAGE&PARTITION CREATOR V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3967,"TEM",1,"Simatic",17,1]
["6AG41141JA210EX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD  WITH PROFINET (3XRJ45, CP1616 COMPATIBLE); 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD-ROM; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS 7 ULTIMATE, 32BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3826,"TEM",1,"Simatic",17,1]
["6AG41141JB211XX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I3-330E (2C/4T, 2.13 GHZ, 3MB CACHE, VT-X, EM64-T); MOTHERBOARD  WITH PROFINET (3XRJ45, CP1616 COMPATIBLE); 500 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD-ROM; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; DVI-VGA-ADAPTER FOR ONBOARD GRAPHICS; WITHOUT OPERATING SYSTEM, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3568,"TEM",1,"Simatic",17,1]
["6AG41141KA120BX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 2 GB DDR3 SDRAM (1 X 2GB), SINGLE CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3143,"TEM",1,"Simatic",17,1]
["6AG41141KA220BX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3406,"TEM",1,"Simatic",17,1]
["6AG41141KD120BX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, 0,5G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 2 GB DDR3 SDRAM (1 X 2GB), SINGLE CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3458,"TEM",1,"Simatic",17,1]
["6AG41141KD121BX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, 0,5G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 2 GB DDR3 SDRAM (1 X 2GB), SINGLE CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; DVI-VGA-ADAPTER FOR ONBOARD GRAPHICS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3484,"TEM",1,"Simatic",17,1]
["6AG41141KG120BX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA; 0,3 G VIBRATION, 3 G SHOCK, INTERNALLY MOUNTED; 2 GB DDR3 SDRAM (1 X 2GB), SINGLE CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3091,"TEM",1,"Simatic",17,1]
["6AG41141KH114EX0","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, REMOVABLE DISK; FRONTSIDE MOUNTED; 2 GB DDR3 SDRAM (1 X 2GB), SINGLE CHANNEL; DVD-ROM; BOARD WITH 11 SLOTS: 7 X PCI, 1 X  PCIE X16, 3 X PCIE X4; WITHOUT HW EXTENSIONS; WINDOWS 7 ULTIMATE, 32BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD EUROPE",3301,"TEM",1,"Simatic",17.25,1]
["6AG41141KM114XX0","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 2 X 500 GB HDD SATA; REMOVABLE DISK; FRONTSIDE MOUNTED; 2 GB DDR3 SDRAM (1 X 2GB), SINGLE CHANNEL; DVD-ROM; BOARD WITH 11 SLOTS: 7 X PCI, 1 X  PCIE X16, 3 X PCIE X4; WITHOUT HW EXTENSIONS; WITHOUT OPERATING SYSTEM, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD EUROPE",3301,"TEM",1,"Simatic",20.059999999999999,1]
["6AG41141KM211XX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 2 X 500 GB HDD SATA; REMOVABLE DISK; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD-ROM; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; DVI-VGA-ADAPTER FOR ONBOARD GRAPHICS; WITHOUT OPERATING SYSTEM, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3453,"TEM",1,"Simatic",17,1]
["6AG41141KP110BX0","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 2 GB DDR3 SDRAM (1 X 2GB), SINGLE CHANNEL; DVD-ROM; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD EUROPE",3574,"TEM",1,"Simatic",17.25,1]
["6AG41141KP110BX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 2 GB DDR3 SDRAM (1 X 2GB), SINGLE CHANNEL; DVD-ROM; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3574,"TEM",1,"Simatic",17.25,1]
["6AG41141KP114EX0","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 2 GB DDR3 SDRAM (1 X 2GB), SINGLE CHANNEL; DVD-ROM; BOARD WITH 11 SLOTS: 7 X PCI, 1 X  PCIE X16, 3 X PCIE X4; WITHOUT HW EXTENSIONS; WINDOWS 7 ULTIMATE, 32BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD EUROPE",3742,"TEM",1,"Simatic",17.25,1]
["6AG41141KP121BX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 2 GB DDR3 SDRAM (1 X 2GB), SINGLE CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; DVI-VGA-ADAPTER FOR ONBOARD GRAPHICS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3684,"TEM",1,"Simatic",17.25,1]
["6AG41141KP220BX5","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD CHINA",3920,"TEM",1,"Simatic",17.25,1]
["6AG41141KP221BX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; DVI-VGA-ADAPTER FOR ONBOARD GRAPHICS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3946,"TEM",1,"Simatic",17.25,1]
["6AG41141KP222BX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16 OCCUPIED; + GRAPHICS CARD PCIE X16, 2 X DP (2 X DVI VIA 2 X DP-DVI-ADAPTER); WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4214,"TEM",1,"Simatic",17.25,1]
["6AG41141KP425QX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM (2 X 4GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 11 SLOTS: 7 X PCI, 1 X  PCIE X16, 3 X PCIE X4; DVI-VGA-ADAPTER FOR ONBOARD GRAPHICS; WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",5458,"TEM",1,"Simatic",17.25,1]
["6AG41141KP610FC6","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM, ECC (2 X 2GB), DUAL CHANNEL; DVD-ROM; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; SIMATIC PC DIAGMONITOR V4.4 & IMAGE&PARTITION CREATOR  V3.3 INCLUDED; 2 X 110/230 IREDUNDANT POWER SUPPLY W/O POWER CORD",4603,"TEM",1,"Simatic",17.25,1]
["6AG41141KR721QA6","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID5 1 TB (3 X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM, ECC (2 X 4GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; DVI-VGA-ADAPTER FOR ONBOARD GRAPHICS; WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1 INCLUDED; SIMATIC PC DIAGMONITOR V4.4 INCLUDED; 2 X 110/230 IREDUNDANT POWER SUPPLY W/O POWER CORD",6361,"TEM",1,"Simatic",17.25,1]
["6AG41141LA222FX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD WITH PROFIBUS/MPI: 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16 OCCUPIED; + GRAPHICS CARD PCIE X16, 2 X DP (2 X DVI VIA 2 X DP-DVI-ADAPTER); WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3941,"TEM",1,"Simatic",17,1]
["6AG41141LB212BA3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD WITH PROFIBUS/MPI: 500 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD-ROM; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16 OCCUPIED; + GRAPHICS CARD PCIE X16, 2 X DP (2 X DVI VIA 2 X DP-DVI-ADAPTER); WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, SIMATIC PC DIAGMONITOR V4.4 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4004,"TEM",1,"Simatic",17,1]
["6AG41141LR620EC6","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I5-520E (2C/4T, 2.4 GHZ, 3MB CACHE,TB,VT-X,VT-D, EM64-T, AMT); MOTHERBOARD WITH PROFIBUS/MPI: RAID5 1 TB (3 X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM, ECC (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS 7 ULTIMATE, 32BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; SIMATIC PC DIAGMONITOR V4.4 & IMAGE&PARTITION CREATOR  V3.3 INCLUDED; 2 X 110/230 IREDUNDANT POWER SUPPLY W/O POWER CORD",5180,"TEM",1,"Simatic",17.25,1]
["6AG41141NA180XX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 2 GB DDR3 SDRAM (1 X 2GB), SINGLE CHANNEL; WITHOUT EXCHANGEABLE MEDIA; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WITHOUT OPERATING SYSTEM, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",2891,"TEM",1,"Simatic",17,1]
["6AG41141NA180XX6","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 2 GB DDR3 SDRAM (1 X 2GB), SINGLE CHANNEL; WITHOUT EXCHANGEABLE MEDIA; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WITHOUT OPERATING SYSTEM, WITHOUT SOFTWARE 2 X 110/230 IREDUNDANT POWER SUPPLY W/O POWER CORD",3311,"TEM",1,"Simatic",17,1]
["6AG41141NB221PX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 500 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; DVI-VGA-ADAPTER FOR ONBOARD GRAPHICS; WINDOWS SERVER 2008 STANDARD EDITION INCL. 5 CLIENT, 32BIT, MUI (EN, GE, FR, IT, SP), SP2; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4524,"TEM",1,"Simatic",17,1]
["6AG41141NB226FX0","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 500 GB HDD SATA, 0,5 G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 11 SLOTS: 7 X PCI, 1XPCIE X16 OCCUPIED, 3XPCIE X4; + GRAPHICS CARD PCIE X16, 2 X DP (2 X DVI VIA 2 X DP-DVI-ADAPTER); WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD EUROPE",4109,"TEM",1,"Simatic",17,1]
["6AG41141ND120BX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, 0,5G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 2 GB DDR3 SDRAM (1 X 2GB), SINGLE CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3647,"TEM",1,"Simatic",17,1]
["6AG41141ND211FC3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, 0,5G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD-ROM; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; DVI-VGA-ADAPTER FOR ONBOARD GRAPHICS; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; SIMATIC PC DIAGMONITOR V4.4 & IMAGE&PARTITION CREATOR  V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4093,"TEM",1,"Simatic",17,1]
["6AG41141ND220BX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, 0,5G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3910,"TEM",1,"Simatic",17,1]
["6AG41141ND225FB0","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, 0,5G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 11 SLOTS: 7 X PCI, 1 X  PCIE X16, 3 X PCIE X4; DVI-VGA-ADAPTER FOR ONBOARD GRAPHICS; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; SIMATIC PC IMAGE&PARTITION CREATOR V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD EUROPE",4188,"TEM",1,"Simatic",17,1]
["6AG41141ND420PX0","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, 0,5G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 8 GB DDR3 SDRAM (2 X 4GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS SERVER 2008 STANDARD EDITION INCL. 5 CLIENT, 32BIT, MUI (EN, GE, FR, IT, SP), SP2; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD EUROPE",5285,"TEM",1,"Simatic",17,1]
["6AG41141ND522PC3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, 0,5G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 2 GB DDR3 SDRAM, ECC (2 X 1GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16 OCCUPIED; + GRAPHICS CARD PCIE X16, 2 X DP (2 X DVI VIA 2 X DP-DVI-ADAPTER); WINDOWS SERVER 2008 STANDARD EDITION INCL. 5 CLIENT, 32BIT, MUI (EN, GE, FR, IT, SP), SP2; SIMATIC PC DIAGMONITOR V4.4 & IMAGE&PARTITION CREATOR  V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",5054,"TEM",1,"Simatic",17,1]
["6AG41141NG014XX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA; 0,3 G VIBRATION, 3 G SHOCK, INTERNALLY MOUNTED; 1 GB DDR3 SDRAM (1 X 1GB), SINGLE CHANNEL; DVD-ROM; BOARD WITH 11 SLOTS: 7 X PCI, 1 X  PCIE X16, 3 X PCIE X4; WITHOUT HW EXTENSIONS; WITHOUT OPERATING SYSTEM, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",2923,"TEM",1,"Simatic",17,1]
["6AG41141NH381BX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, REMOVABLE DISK; FRONTSIDE MOUNTED; 6 GB DDR3 SDRAM (1X2GB, 1X4GB), DUAL CHANNEL; WITHOUT EXCHANGEABLE MEDIA; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; DVI-VGA-ADAPTER FOR ONBOARD GRAPHICS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3820,"TEM",1,"Simatic",17.25,1]
["6AG41141NH421EX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 250 GB HDD SATA, REMOVABLE DISK; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM (2 X 4GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; DVI-VGA-ADAPTER FOR ONBOARD GRAPHICS; WINDOWS 7 ULTIMATE, 32BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4251,"TEM",1,"Simatic",17.25,1]
["6AG41141NM211QB3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; 2 X 500 GB HDD SATA; REMOVABLE DISK; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD-ROM; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; DVI-VGA-ADAPTER FOR ONBOARD GRAPHICS; WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1 INCLUDED; SIMATIC PC IMAGE&PARTITION CREATOR V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4881,"TEM",1,"Simatic",17,1]
["6AG41141NP210NX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD-ROM; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS SERVER 2003 R2 STANDARD EDITION INCL. 5 CLIENT, 32BIT, MUI (EN, GE, FR, IT, SP),SP2; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4876,"TEM",1,"Simatic",17.25,1]
["6AG41141NP210NX6","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD-ROM; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS SERVER 2003 R2 STANDARD EDITION INCL. 5 CLIENT, 32BIT, MUI (EN, GE, FR, IT, SP),SP2; WITHOUT SOFTWARE 2 X 110/230 IREDUNDANT POWER SUPPLY W/O POWER CORD",5296,"TEM",1,"Simatic",17.25,1]
["6AG41141NP220BX5","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD CHINA",4109,"TEM",1,"Simatic",17.25,1]
["6AG41141NP221PX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; DVI-VGA-ADAPTER FOR ONBOARD GRAPHICS; WINDOWS SERVER 2008 STANDARD EDITION INCL. 5 CLIENT, 32BIT, MUI (EN, GE, FR, IT, SP), SP2; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4986,"TEM",1,"Simatic",17.25,1]
["6AG41141NP222PA3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16 OCCUPIED; + GRAPHICS CARD PCIE X16, 2 X DP (2 X DVI VIA 2 X DP-DVI-ADAPTER); WINDOWS SERVER 2008 STANDARD EDITION INCL. 5 CLIENT, 32BIT, MUI (EN, GE, FR, IT, SP), SP2; SIMATIC PC DIAGMONITOR V4.4 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",5380,"TEM",1,"Simatic",17.25,1]
["6AG41141NP222PA6","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16 OCCUPIED; + GRAPHICS CARD PCIE X16, 2 X DP (2 X DVI VIA 2 X DP-DVI-ADAPTER); WINDOWS SERVER 2008 STANDARD EDITION INCL. 5 CLIENT, 32BIT, MUI (EN, GE, FR, IT, SP), SP2; SIMATIC PC DIAGMONITOR V4.4 INCLUDED; 2 X 110/230 IREDUNDANT POWER SUPPLY W/O POWER CORD",5800,"TEM",1,"Simatic",17.25,1]
["6AG41141NP285EX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; WITHOUT EXCHANGEABLE MEDIA; BOARD WITH 11 SLOTS: 7 X PCI, 1 X  PCIE X16, 3 X PCIE X4; DVI-VGA-ADAPTER FOR ONBOARD GRAPHICS; WINDOWS 7 ULTIMATE, 32BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4167,"TEM",1,"Simatic",17.25,1]
["6AG41141NP416QC3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM (2 X 4GB), DUAL CHANNEL; DVD-ROM; BOARD WITH 11 SLOTS: 7 X PCI, 1XPCIE X16 OCCUPIED, 3XPCIE X4; + GRAPHICS CARD PCIE X16, 2 X DP (2 X DVI VIA 2 X DP-DVI-ADAPTER); WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1 INCLUDED; SIMATIC PC DIAGMONITOR V4.4 & IMAGE&PARTITION CREATOR  V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",6041,"TEM",1,"Simatic",17.25,1]
["6AG41141NP510FX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 2 GB DDR3 SDRAM, ECC (2 X 1GB), DUAL CHANNEL; DVD-ROM; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3847,"TEM",1,"Simatic",17.25,1]
["6AG41141NP522NC3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 2 GB DDR3 SDRAM, ECC (2 X 1GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16 OCCUPIED; + GRAPHICS CARD PCIE X16, 2 X DP (2 X DVI VIA 2 X DP-DVI-ADAPTER); WINDOWS SERVER 2003 R2 STANDARD EDITION INCL. 5 CLIENT, 32BIT, MUI (EN, GE, FR, IT, SP),SP2; SIMATIC PC DIAGMONITOR V4.4 & IMAGE&PARTITION CREATOR  V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",5254,"TEM",1,"Simatic",17.25,1]
["6AG41141NP624XX0","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM, ECC (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 11 SLOTS: 7 X PCI, 1 X  PCIE X16, 3 X PCIE X4; WITHOUT HW EXTENSIONS; WITHOUT OPERATING SYSTEM, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD EUROPE",4046,"TEM",1,"Simatic",17.25,1]
["6AG41141NP724QA6","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM, ECC (2 X 4GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 11 SLOTS: 7 X PCI, 1 X  PCIE X16, 3 X PCIE X4; WITHOUT HW EXTENSIONS; WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1 INCLUDED; SIMATIC PC DIAGMONITOR V4.4 INCLUDED; 2 X 110/230 IREDUNDANT POWER SUPPLY W/O POWER CORD",6377,"TEM",1,"Simatic",17.25,1]
["6AG41141NR210XX6","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID5 1 TB (3 X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD-ROM; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WITHOUT OPERATING SYSTEM, WITHOUT SOFTWARE 2 X 110/230 IREDUNDANT POWER SUPPLY W/O POWER CORD",4424,"TEM",1,"Simatic",17.25,1]
["6AG41141NR220EC3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID5 1 TB (3 X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS 7 ULTIMATE, 32BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; SIMATIC PC DIAGMONITOR V4.4 & IMAGE&PARTITION CREATOR  V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4634,"TEM",1,"Simatic",17.25,1]
["6AG41141NR420BC3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID5 1 TB (3 X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM (2 X 4GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, SIMATIC PC DIAGMONITOR V4.4 & IMAGE&PARTITION CREATOR  V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",5128,"TEM",1,"Simatic",17.25,1]
["6AG41141NR626XX6","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID5 1 TB (3 X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM, ECC (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 11 SLOTS: 7 X PCI, 1XPCIE X16 OCCUPIED, 3XPCIE X4; + GRAPHICS CARD PCIE X16, 2 X DP (2 X DVI VIA 2 X DP-DVI-ADAPTER); WITHOUT OPERATING SYSTEM, WITHOUT SOFTWARE 2 X 110/230 IREDUNDANT POWER SUPPLY W/O POWER CORD",5044,"TEM",1,"Simatic",17.25,1]
["6AG41141NR720PC6","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID5 1 TB (3 X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM, ECC (2 X 4GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS SERVER 2008 STANDARD EDITION INCL. 5 CLIENT, 32BIT, MUI (EN, GE, FR, IT, SP), SP2; SIMATIC PC DIAGMONITOR V4.4 & IMAGE&PARTITION CREATOR  V3.3 INCLUDED; 2 X 110/230 IREDUNDANT POWER SUPPLY W/O POWER CORD",6608,"TEM",1,"Simatic",17.25,1]
["6AG41141NU224PC0","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD W/O FIELDBUS; RAID1 1TB (2 X 1 TB HDD SAS), REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; PCIE X8 RAID CONTROLLER IN PCIE X16 SLOT; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 11 SLOTS: 7 X PCI, 1 X  PCIE X16, 3 X PCIE X4; WITHOUT HW EXTENSIONS; WINDOWS SERVER 2008 STANDARD EDITION INCL. 5 CLIENT, 32BIT, MUI (EN, GE, FR, IT, SP), SP2; SIMATIC PC DIAGMONITOR V4.4 & IMAGE&PARTITION CREATOR  V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD EUROPE",6829,"TEM",1,"Simatic",17.25,1]
["6AG41141PD210BX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD WITH PROFIBUS/MPI: RAID1 500GB (2X 500GB HDD SATA, 0,5G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD-ROM; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",4036,"TEM",1,"Simatic",17,1]
["6AG41141PD227NC3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD WITH PROFIBUS/MPI: RAID1 500GB (2X 500GB HDD SATA, 0,5G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 11 SLOTS: 7 X PCI, 1XPCIE X16 OCCUPIED, 3XPCIE X4; + GRAPHICS CARD PCIE X16, 2 X DP (2 X VGA VIA 2 X DP-VGA-ADAPTER); WINDOWS SERVER 2003 R2 STANDARD EDITION INCL. 5 CLIENT, 32BIT, MUI (EN, GE, FR, IT, SP),SP2; SIMATIC PC DIAGMONITOR V4.4 & IMAGE&PARTITION CREATOR  V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",5653,"TEM",1,"Simatic",17,1]
["6AG41141PD625BB0","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD WITH PROFIBUS/MPI: RAID1 500GB (2X 500GB HDD SATA, 0,5G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM, ECC (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 11 SLOTS: 7 X PCI, 1 X  PCIE X16, 3 X PCIE X4; DVI-VGA-ADAPTER FOR ONBOARD GRAPHICS; WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, SIMATIC PC IMAGE&PARTITION CREATOR V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD EUROPE",4471,"TEM",1,"Simatic",17,1]
["6AG41141PG214EX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD WITH PROFIBUS/MPI: 250 GB HDD SATA; 0,3 G VIBRATION, 3 G SHOCK, INTERNALLY MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD-ROM; BOARD WITH 11 SLOTS: 7 X PCI, 1 X  PCIE X16, 3 X PCIE X4; WITHOUT HW EXTENSIONS; WINDOWS 7 ULTIMATE, 32BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",3836,"TEM",1,"Simatic",17,1]
["6AG41141PM221QX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD WITH PROFIBUS/MPI: 2 X 500 GB HDD SATA; REMOVABLE DISK; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; DVI-VGA-ADAPTER FOR ONBOARD GRAPHICS; WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",5091,"TEM",1,"Simatic",17,1]
["6AG41141PR722BC3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD WITH PROFIBUS/MPI: RAID5 1 TB (3 X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM, ECC (2 X 4GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16 OCCUPIED; + GRAPHICS CARD PCIE X16, 2 X DP (2 X DVI VIA 2 X DP-DVI-ADAPTER); WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, SIMATIC PC DIAGMONITOR V4.4 & IMAGE&PARTITION CREATOR  V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",5842,"TEM",1,"Simatic",17.25,1]
["6AG41141PV224PX6","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD WITH PROFIBUS/MPI: RAID5 1,8TB (3 X 1 TB HDD SAS), REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; PCIE X8 RAID CONTROLLER IN PCIE X16 SLOT; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 11 SLOTS: 7 X PCI, 1 X  PCIE X16, 3 X PCIE X4; WITHOUT HW EXTENSIONS; WINDOWS SERVER 2008 STANDARD EDITION INCL. 5 CLIENT, 32BIT, MUI (EN, GE, FR, IT, SP), SP2; WITHOUT SOFTWARE 2 X 110/230 IREDUNDANT POWER SUPPLY W/O POWER CORD",7774,"TEM",1,"Simatic",17.25,1]
["6AG41141RD721EA4","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD WITH PROFINET (3XRJ45, CP1616 COMPATIBLE); RAID1 500GB (2X 500GB HDD SATA, 0,5G VIBRATION, 5 G SHOCK, INTERNALLY MOUNTED; 8 GB DDR3 SDRAM, ECC (2 X 4GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; DVI-VGA-ADAPTER FOR ONBOARD GRAPHICS; WINDOWS 7 ULTIMATE, 32BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; SIMATIC PC DIAGMONITOR V4.4 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD ITALY",5437,"TEM",1,"Simatic",17,1]
["6AG41141RP622EC3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD WITH PROFINET (3XRJ45, CP1616 COMPATIBLE); RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM, ECC (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16 OCCUPIED; + GRAPHICS CARD PCIE X16, 2 X DP (2 X DVI VIA 2 X DP-DVI-ADAPTER); WINDOWS 7 ULTIMATE, 32BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; SIMATIC PC DIAGMONITOR V4.4 & IMAGE&PARTITION CREATOR  V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",5359,"TEM",1,"Simatic",17.25,1]
["6AG41141RP720EX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD WITH PROFINET (3XRJ45, CP1616 COMPATIBLE); RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM, ECC (2 X 4GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS 7 ULTIMATE, 32BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",5485,"TEM",1,"Simatic",17.25,1]
["6AG41141RP720FX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD WITH PROFINET (3XRJ45, CP1616 COMPATIBLE); RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM, ECC (2 X 4GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",5485,"TEM",1,"Simatic",17.25,1]
["6AG41141RP720FX5","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD WITH PROFINET (3XRJ45, CP1616 COMPATIBLE); RAID1 500GB (2X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM, ECC (2 X 4GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 8 SLOTS: 7 X PCI, 1 X  PCIE X16; WITHOUT HW EXTENSIONS; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD CHINA",5485,"TEM",1,"Simatic",17.25,1]
["6AG41141RR224EX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD WITH PROFINET (3XRJ45, CP1616 COMPATIBLE); RAID5 1 TB (3 X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2 X 2GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 11 SLOTS: 7 X PCI, 1 X  PCIE X16, 3 X PCIE X4; WITHOUT HW EXTENSIONS; WINDOWS 7 ULTIMATE, 32BIT, MUI (EN, GER, FR, IT, SP), SP1 INCLUDED; WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",5170,"TEM",1,"Simatic",17.25,1]
["6AG41141RR726BX3","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD WITH PROFINET (3XRJ45, CP1616 COMPATIBLE); RAID5 1 TB (3 X 500GB HDD SATA, REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM, ECC (2 X 4GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 11 SLOTS: 7 X PCI, 1XPCIE X16 OCCUPIED, 3XPCIE X4; + GRAPHICS CARD PCIE X16, 2 X DP (2 X DVI VIA 2 X DP-DVI-ADAPTER); WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, WITHOUT SOFTWARE 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD USA",6167,"TEM",1,"Simatic",17.25,1]
["6AG41141RS727BC5","SIMATIC IPC847C (RACK PC, 19\", 4U); INTERFACES:2 X GBIT LAN (RJ45); 1 X DVI-I; AUDIO; 2 X COM; 1 X LPT; 2 X PS/2; 4 X USB 2.0 BACKSIDE, 2 X USB 2.0 FRONTSIDE; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I7-610E (2C/4T, 2.53 GHZ, 4MB CACHE, TB, VT-X,VT-D, EM64-T, AMT); MOTHERBOARD WITH PROFINET (3XRJ45, CP1616 COMPATIBLE); 50 GB SSD SATA; INTERNALLY MOUNTED; 8 GB DDR3 SDRAM, ECC (2 X 4GB), DUAL CHANNEL; DVD +/- RW; BOARD WITH 11 SLOTS: 7 X PCI, 1XPCIE X16 OCCUPIED, 3XPCIE X4; + GRAPHICS CARD PCIE X16, 2 X DP (2 X VGA VIA 2 X DP-VGA-ADAPTER); WINDOWS XP PROFESSIONAL, 32BIT, MUI (EN, GER, FR, IT, SP), SP3, SIMATIC PC DIAGMONITOR V4.4 & IMAGE&PARTITION CREATOR  V3.3 INCLUDED; 110/230 INDUSTRIAL POWER SUPPLY WITH NAMUR; PS CORD CHINA",6083,"TEM",1,"Simatic",17,1]
["6AG41142DJ321BB3","SIMATIC IPC847D (RACK PC) (RACK PC, 19\", 4U); 2X GBIT ETHERNET (IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0 INCL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I3-4330TE (2C/4T, 2.4GHZ, 4MB CACHE); MAINBOARD W/O FIELDBUS; RAID1, 1 TB (2X 1 TB HDD SATA, DATA MIRRORING), REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM (2X 4GB), DUAL CHANNEL; BOARD WITH 11 SLOTS: 7X PCI, 3X PCIE X4, 1X PCIE X16; DVD +/- RW (SLIM); W/O EXTENSION (HW); GRAPHICS ONBOARD; ADAPTER CABLE DVI-I TO VGA FOR ONBOARD GRAPHICS; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; SIMATIC PC IMAGE&PARTITION CREATOR V3.4 INCLUDED; 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD USA",3523,"TEM",1,"Simatic",17,1]
["6AG41142GJ202BX0","SIMATIC IPC847D (RACK PC) (RACK PC, 19\", 4U); 2X GBIT ETHERNET (IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0 INCL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I5-4570TE (2C/4T, 2.7(3.3) GHZ, 4MB CACHE, TB,VT-D, AMT); MAINBOARD W/O FELDBUS; RAID1, 1 TB (2X 1 TB HDD SATA, DATA MIRRORING), REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2X 2GB), DUAL CHANNEL; BOARD WITH 11 SLOTS: 7X PCI, 3X PCIE X4, 1X PCIE X16; WITHOUT HW EXTENSIONS; COM2; LPT (1 SLOT OCCUPIED); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; WITHOUT EXTENSION (SW); 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD EUROPE",3318,"TEM",1,"Simatic",17,1]
["6AG41142GJ222BX0","SIMATIC IPC847D (RACK PC) (RACK PC, 19\", 4U); 2X GBIT ETHERNET (IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0 INCL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I5-4570TE (2C/4T, 2.7(3.3) GHZ, 4MB CACHE, TB,VT-D, AMT); MAINBOARD W/O FELDBUS; RAID1, 1 TB (2X 1 TB HDD SATA, DATA MIRRORING), REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2X 2GB), DUAL CHANNEL; BOARD WITH 11 SLOTS: 7X PCI, 3X PCIE X4, 1X PCIE X16; DVD +/- RW (SLIM); COM2; LPT (1 SLOT OCCUPIED); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; WITHOUT EXTENSION (SW); 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD EUROPE",3455,"TEM",1,"Simatic",17,1]
["6AG41142GN202BX0","SIMATIC IPC847D (RACK PC) (RACK PC, 19\", 4U); 2X GBIT ETHERNET (IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0 INCL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I5-4570TE (2C/4T, 2.7(3.3) GHZ, 4MB CACHE, TB,VT-D, AMT); MAINBOARD W/O FELDBUS; 240 GB SSD SATA, REMOVABLE DISK; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2X 2GB), DUAL CHANNEL; BOARD WITH 11 SLOTS: 7X PCI, 3X PCIE X4, 1X PCIE X16; WITHOUT HW EXTENSIONS; COM2; LPT (1 SLOT OCCUPIED); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; WITHOUT EXTENSION (SW); 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD EUROPE",3392,"TEM",1,"Simatic",17.25,1]
["6AG41142GN222BX0","SIMATIC IPC847D (RACK PC) (RACK PC, 19\", 4U); 2X GBIT ETHERNET (IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0 INCL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER CORE I5-4570TE (2C/4T, 2.7(3.3) GHZ, 4MB CACHE, TB,VT-D, AMT); MAINBOARD W/O FELDBUS; 240 GB SSD SATA, REMOVABLE DISK; FRONTSIDE MOUNTED; 4 GB DDR3 SDRAM (2X 2GB), DUAL CHANNEL; BOARD WITH 11 SLOTS: 7X PCI, 3X PCIE X4, 1X PCIE X16; DVD +/- RW (SLIM); COM2; LPT (1 SLOT OCCUPIED); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; WITHOUT EXTENSION (SW); 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD EUROPE",3528,"TEM",1,"Simatic",17.25,1]
["6AG41142KE710FX3","SIMATIC IPC847D (RACK PC) (RACK PC, 19\", 4U); 2X GBIT ETHERNET (IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0 INCL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER XEON E3-1268LV3 (4C/8T, 2.3(3.3) GHZ, 8MB CACHE VT-D, AMT); MAINBOARD W/O FELDBUS; RAID1, 1 TB (2X 1 TB HDD SATA, DATA MIRRORING), INTERNALLY MOUNTED; 0,5G VIBRATION, 5 G SHOCK, 16 GB DDR3 SDRAM (2X 8GB), ECC, DUAL CHANNEL; BOARD WITH 11 SLOTS: 3X PCI, 3X PCIE X4, 5X PCIE X16; WITHOUT HW EXTENSIONS; W/O EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; WITHOUT EXTENSION (SW); 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD USA",5093,"TEM",1,"Simatic",17,1]
["6AG41142KJ302BX0","SIMATIC IPC847D (RACK PC) (RACK PC, 19\", 4U); 2X GBIT ETHERNET (IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0 INCL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER XEON E3-1268LV3 (4C/8T, 2.3(3.3) GHZ, 8MB CACHE VT-D, AMT); MAINBOARD W/O FELDBUS; RAID1, 1 TB (2X 1 TB HDD SATA, DATA MIRRORING), REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM (2X 4GB), DUAL CHANNEL; BOARD WITH 11 SLOTS: 7X PCI, 3X PCIE X4, 1X PCIE X16; WITHOUT HW EXTENSIONS; COM2; LPT (1 SLOT OCCUPIED); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; WITHOUT EXTENSION (SW); 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD EUROPE",3759,"TEM",1,"Simatic",17,1]
["6AG41142KJ320BA3","SIMATIC IPC847D (RACK PC) (RACK PC, 19\", 4U); 2X GBIT ETHERNET (IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0 INCL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER XEON E3-1268LV3 (4C/8T, 2.3(3.3) GHZ, 8MB CACHE VT-D, AMT); MAINBOARD W/O FELDBUS; RAID1, 1 TB (2X 1 TB HDD SATA, DATA MIRRORING), REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM (2X 4GB), DUAL CHANNEL; BOARD WITH 11 SLOTS: 7X PCI, 3X PCIE X4, 1X PCIE X16; DVD +/- RW (SLIM); W/O EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; SIMATIC PC DIAGMONITOR V4.5 INCLUDED; 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD USA",3959,"TEM",1,"Simatic",17,1]
["6AG41142KJ322BX0","SIMATIC IPC847D (RACK PC) (RACK PC, 19\", 4U); 2X GBIT ETHERNET (IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0 INCL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER XEON E3-1268LV3 (4C/8T, 2.3(3.3) GHZ, 8MB CACHE VT-D, AMT); MAINBOARD W/O FELDBUS; RAID1, 1 TB (2X 1 TB HDD SATA, DATA MIRRORING), REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM (2X 4GB), DUAL CHANNEL; BOARD WITH 11 SLOTS: 7X PCI, 3X PCIE X4, 1X PCIE X16; DVD +/- RW (SLIM); COM2; LPT (1 SLOT OCCUPIED); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; WITHOUT EXTENSION (SW); 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD EUROPE",3896,"TEM",1,"Simatic",17,1]
["6AG41142KM410BX0","SIMATIC IPC847D (RACK PC) (RACK PC, 19\", 4U); 2X GBIT ETHERNET (IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0 INCL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER XEON E3-1268LV3 (4C/8T, 2.3(3.3) GHZ, 8MB CACHE VT-D, AMT); MAINBOARD W/O FELDBUS; 240 GB SSD SATA, INTERNALLY MOUNTED; 16 GB DDR3 SDRAM (2X 8GB), DUAL CHANNEL; BOARD WITH 11 SLOTS: 3X PCI, 3X PCIE X4, 5X PCIE X16; WITHOUT HW EXTENSIONS; W/O EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; WITHOUT EXTENSION (SW); 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD EUROPE",4085,"TEM",1,"Simatic",17,1]
["6AG41142KN302BX0","SIMATIC IPC847D (RACK PC) (RACK PC, 19\", 4U); 2X GBIT ETHERNET (IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0 INCL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER XEON E3-1268LV3 (4C/8T, 2.3(3.3) GHZ, 8MB CACHE VT-D, AMT); MAINBOARD W/O FELDBUS; 240 GB SSD SATA, REMOVABLE DISK; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM (2X 4GB), DUAL CHANNEL; BOARD WITH 11 SLOTS: 7X PCI, 3X PCIE X4, 1X PCIE X16; WITHOUT HW EXTENSIONS; COM2; LPT (1 SLOT OCCUPIED); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; WITHOUT EXTENSION (SW); 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD EUROPE",3833,"TEM",1,"Simatic",17.25,1]
["6AG41142KN322BX0","SIMATIC IPC847D (RACK PC) (RACK PC, 19\", 4U); 2X GBIT ETHERNET (IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0 INCL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER XEON E3-1268LV3 (4C/8T, 2.3(3.3) GHZ, 8MB CACHE VT-D, AMT); MAINBOARD W/O FELDBUS; 240 GB SSD SATA, REMOVABLE DISK; FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM (2X 4GB), DUAL CHANNEL; BOARD WITH 11 SLOTS: 7X PCI, 3X PCIE X4, 1X PCIE X16; DVD +/- RW (SLIM); COM2; LPT (1 SLOT OCCUPIED); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; WITHOUT EXTENSION (SW); 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD EUROPE",3969,"TEM",1,"Simatic",17.25,1]
["6AG41142KN522BX5","SIMATIC IPC847D (RACK PC) (RACK PC, 19\", 4U); 2X GBIT ETHERNET (IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0 INCL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER XEON E3-1268LV3 (4C/8T, 2.3(3.3) GHZ, 8MB CACHE VT-D, AMT); MAINBOARD W/O FELDBUS; 240 GB SSD SATA, REMOVABLE DISK; FRONTSIDE MOUNTED; 32 GB DDR3 SDRAM (4X 8GB), DUAL CHANNEL; BOARD WITH 11 SLOTS: 7X PCI, 3X PCIE X4, 1X PCIE X16; DVD +/- RW (SLIM); COM2; LPT (1 SLOT OCCUPIED); GRAPHICS ONBOARD; WINDOWS 7 ULTIMATE, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; WITHOUT EXTENSION (SW); 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD CHINA",4967,"TEM",1,"Simatic",17.25,1]
["6AG41142KQ730FX6","SIMATIC IPC847D (RACK PC) (RACK PC, 19\", 4U); 2X GBIT ETHERNET (IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0 INCL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER XEON E3-1268LV3 (4C/8T, 2.3(3.3) GHZ, 8MB CACHE VT-D, AMT); MAINBOARD W/O FELDBUS; RAID1, 1 TB (2X 1 TB HDD SATA, DATA MIRRORING), REMOVABLE DISK, HOT-SWAP; FRONTSIDE MOUNTED; AND 1 TB HDD SATA  AS HOT-SPARE REMOVABLE DISK, FRONTSIDE  MOUNTED; 16 GB DDR3 SDRAM (2X 8GB), ECC, DUAL CHANNEL; BOARD WITH 11 SLOTS: 3X PCI, 3X PCIE X4, 5X PCIE X16; DVD +/- RW (SLIM); W/O EXTENSION (HW); GRAPHICS ONBOARD; WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; WITHOUT EXTENSION (SW); 2 X 110/240V REDUNDANT POWER SUPPLY W/O POWER CORD",6279,"TEM",1,"Simatic",17,1]
["6AG41142KR400XA3","SIMATIC IPC847D (RACK PC) (RACK PC, 19\", 4U); 2X GBIT ETHERNET (IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0 INCL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER XEON E3-1268LV3 (4C/8T, 2.3(3.3) GHZ, 8MB CACHE VT-D, AMT); MAINBOARD W/O FELDBUS; RAID1, 1 TB (2X 1 TB HDD SATA, DATA MIRRORING), REMOVABLE DISK, HOT-SWAP; AND 240 GB SSD SATA (FOR OPERTING SYSTEM) REMOVABLE DISK, FRONTSIDE MOUNTED; 16 GB DDR3 SDRAM (2X 8GB), DUAL CHANNEL; BOARD WITH 11 SLOTS: 7X PCI, 3X PCIE X4, 1X PCIE X16; WITHOUT HW EXTENSIONS; W/O EXTENSION (HW); GRAPHICS ONBOARD; WITHOUT OPERATING SYSTEM, SIMATIC PC DIAGMONITOR V4.5 INCLUDED; 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD USA",4715,"TEM",1,"Simatic",17,1]
["6AG41142LE523FX6","SIMATIC IPC847D (RACK PC) (RACK PC, 19\", 4U); 2X GBIT ETHERNET (IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0 INCL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER XEON E3-1268LV3 (4C/8T, 2.3(3.3) GHZ, 8MB CACHE VT-D, AMT); MAINBOARD WITH PROFIBUS/MPI (CP5622-COMPATIBLE); RAID1, 1 TB (2X 1 TB HDD SATA, DATA MIRRORING), INTERNALLY MOUNTED; 0,5G VIBRATION, 5 G SHOCK, 32 GB DDR3 SDRAM (4X 8GB), DUAL CHANNEL; BOARD WITH 11 SLOTS: 7X PCI, 3X PCIE X4, 1X PCIE X16; DVD +/- RW (SLIM); COM2; LPT (1 SLOT OCCUPIED); GRAPHICS ONBOARD; ADAPTER CABLE DVI-I TO VGA FOR ONBOARD GRAPHICS; WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; WITHOUT EXTENSION (SW); 2 X 110/240V REDUNDANT POWER SUPPLY W/O POWER CORD",6169,"TEM",1,"Simatic",17,1]
["6AG41142LH504FX3","SIMATIC IPC847D (RACK PC) (RACK PC, 19\", 4U); 2X GBIT ETHERNET (IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0 INCL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER XEON E3-1268LV3 (4C/8T, 2.3(3.3) GHZ, 8MB CACHE VT-D, AMT); MAINBOARD WITH PROFIBUS/MPI (CP5622-COMPATIBLE); 2X 1 TB HDD SATA, REMOVABLE DISK; FRONTSIDE MOUNTED; 32 GB DDR3 SDRAM (4X 8GB), DUAL CHANNEL; BOARD WITH 11 SLOTS: 7X PCI, 3X PCIE X4, 1X PCIE X16; WITHOUT HW EXTENSIONS; COM2; LPT (1 SLOT OCCUPIED); +PCIE X16 GRAPHICS CARD (DUAL HEAD: 2X VGA OR 2X DVI-D), 512MB, (1 SLOT OCCUPIED); WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; WITHOUT EXTENSION (SW); 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD USA",5975,"TEM",1,"Simatic",17.25,1]
["6AG41142ML434FC3","SIMATIC IPC847D (RACK PC) (RACK PC, 19\", 4U); 2X GBIT ETHERNET (IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0 INCL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER XEON E3-1268LV3 (4C/8T, 2.3(3.3) GHZ, 8MB CACHE VT-D, AMT); MAINBOARD WITH PROFINET (3X RJ45, CP1616-COMPATIBLE); RAID5, 2 TB (3X 1 TB HDD SATA, STRIPING WITH PARITY), REMOVABLE DISK, HOT-SWAP; AND 1 TB HDD SATA AS HOT-SPARE REMOVABLE DISK, FRONTSIDE MOUNTED; 16 GB DDR3 SDRAM (2X 8GB), DUAL CHANNEL; BOARD WITH 11 SLOTS: 3X PCI, 3X PCIE X4, 5X PCIE X16; DVD +/- RW (SLIM); COM2; LPT (1 SLOT OCCUPIED); +PCIE X16 GRAPHICS CARD (DUAL HEAD: 2X VGA OR 2X DVI-D), 512MB, (1 SLOT OCCUPIED); WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; SIMATIC PC DIAGMONITOR V4.5 AND IMAGE&PARTITION CREATOR  V3.4 INCLUDED; 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD USA",6993,"TEM",1,"Simatic",17,1]
["6AG41142ML523FC3","SIMATIC IPC847D (RACK PC) (RACK PC, 19\", 4U); 2X GBIT ETHERNET (IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0 INCL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER XEON E3-1268LV3 (4C/8T, 2.3(3.3) GHZ, 8MB CACHE VT-D, AMT); MAINBOARD WITH PROFINET (3X RJ45, CP1616-COMPATIBLE); RAID5, 2 TB (3X 1 TB HDD SATA, STRIPING WITH PARITY), REMOVABLE DISK, HOT-SWAP; AND 1 TB HDD SATA AS HOT-SPARE REMOVABLE DISK, FRONTSIDE MOUNTED; 32 GB DDR3 SDRAM (4X 8GB), DUAL CHANNEL; BOARD WITH 11 SLOTS: 7X PCI, 3X PCIE X4, 1X PCIE X16; DVD +/- RW (SLIM); COM2; LPT (1 SLOT OCCUPIED); GRAPHICS ONBOARD; ADAPTER CABLE DVI-I TO VGA FOR ONBOARD GRAPHICS; WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; SIMATIC PC DIAGMONITOR V4.5 AND IMAGE&PARTITION CREATOR  V3.4 INCLUDED; 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD USA",7282,"TEM",1,"Simatic",17,1]
["6AG41142MR322FA3","SIMATIC IPC847D (RACK PC) (RACK PC, 19\", 4U); 2X GBIT ETHERNET (IE/PN), RJ45; 1X DVI-I; 2X DISPLAYPORT; 1X COM1; 2X PS/2; AUDIO; 4X USB 3.0 INCL.1X INTERNALLY; 3X USB 2.0; TEMPERATURE AND FAN CONTROL; WATCHDOG; BOARD RETAINER XEON E3-1268LV3 (4C/8T, 2.3(3.3) GHZ, 8MB CACHE VT-D, AMT); MAINBOARD WITH PROFINET (3X RJ45, CP1616-COMPATIBLE); RAID1, 1 TB (2X 1 TB HDD SATA, DATA MIRRORING), REMOVABLE DISK, HOT-SWAP; AND 240 GB SSD SATA (FOR OPERTING SYSTEM) REMOVABLE DISK, FRONTSIDE MOUNTED; 8 GB DDR3 SDRAM (2X 4GB), DUAL CHANNEL; BOARD WITH 11 SLOTS: 7X PCI, 3X PCIE X4, 1X PCIE X16; DVD +/- RW (SLIM); COM2; LPT (1 SLOT OCCUPIED); GRAPHICS ONBOARD; WINDOWS SERVER 2008 R2 STANDARD EDITION INCL. 5 CLIENT, 64BIT, MUI (EN, GE, FR, IT, SP), SP1; SIMATIC PC DIAGMONITOR V4.5 INCLUDED; 110/240V INDUSTR. POWER SUPPLY WITH NAMUR; PS CORD USA",6342,"TEM",1,"Simatic",17,1]
["6AG41312AB122AX6","SIMATIC IPC627D (BOX PC), HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; CELERON G1820TE (2C/2T, 2.2GHZ, 2MB CACHE); 250 GB HDD SATA; DVD+/-RW; 2 GB DDR3 1600 DIMM; 1 X PCIE (X16); 1 X PCIE (X4); COM2; LPT (1 SLOT OCCUPIED); WINDOWS 7 ULTIMATE 32BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); DC 24V  INDUSTRAL- POWER SUPPLY;",2590,"TEM",1,"Simatic",6,1]
["6AG41312AB222AX6","SIMATIC IPC627D (BOX PC), HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; CELERON G1820TE (2C/2T, 2.2GHZ, 2MB CACHE); 250 GB HDD SATA; DVD+/-RW; 4 GB DDR3 1600 DIMM; 1 X PCIE (X16); 1 X PCIE (X4); COM2; LPT (1 SLOT OCCUPIED); WINDOWS 7 ULTIMATE 32BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); DC 24V  INDUSTRAL- POWER SUPPLY;",2674,"TEM",1,"Simatic",6,1]
["6AG41312AB222BX6","SIMATIC IPC627D (BOX PC), HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; CELERON G1820TE (2C/2T, 2.2GHZ, 2MB CACHE); 250 GB HDD SATA; DVD+/-RW; 4 GB DDR3 1600 DIMM; 1 X PCIE (X16); 1 X PCIE (X4); COM2; LPT (1 SLOT OCCUPIED); WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); DC 24V  INDUSTRAL- POWER SUPPLY;",2674,"TEM",1,"Simatic",6,1]
["6AG41312AB322BX6","SIMATIC IPC627D (BOX PC), HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; CELERON G1820TE (2C/2T, 2.2GHZ, 2MB CACHE); 250 GB HDD SATA; DVD+/-RW; 8 GB DDR3 1600 DIMM; 1 X PCIE (X16); 1 X PCIE (X4); COM2; LPT (1 SLOT OCCUPIED); WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); DC 24V  INDUSTRAL- POWER SUPPLY;",2821,"TEM",1,"Simatic",6,1]
["6AG41312CM200AX3","SIMATIC IPC627D (BOX PC), HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; CELERON G1820TE (2C/2T, 2.2GHZ, 2MB CACHE); PROFINET (IRT, 3 PORTS, CP1616-COMPATIBLE); 2 MB BUFFERED SRAM; SOLID STATE DRIVE 240 GB; 4 GB DDR3 1600 DIMM; 2 X  PCI; W/O EXTENSION (HW); WINDOWS 7 ULTIMATE 32BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); AC 110/230V INDUSTRIAL POWER SUPPLY WITH NAMUR; POWER CORD USA;",3356,"TEM",1,"Simatic",6,1]
["6AG41312DB122AX6","SIMATIC IPC627D (BOX PC), HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; CORE I3-4330TE (2C/4T, 2.4GHZ, 4MB CACHE, VT-X); 250 GB HDD SATA; DVD+/-RW; 2 GB DDR3 1600 DIMM; 1 X PCIE (X16); 1 X PCIE (X4); COM2; LPT (1 SLOT OCCUPIED); WINDOWS 7 ULTIMATE 32BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); DC 24V  INDUSTRAL- POWER SUPPLY;",2873,"TEM",1,"Simatic",6,1]
["6AG41312DB200BX6","SIMATIC IPC627D (BOX PC), HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; CORE I3-4330TE (2C/4T, 2.4GHZ, 4MB CACHE, VT-X); 250 GB HDD SATA; DVD+/-RW; 4 GB DDR3 1600 DIMM; 2 X  PCI; W/O EXTENSION (HW); WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); DC 24V  INDUSTRAL- POWER SUPPLY;",2821,"TEM",1,"Simatic",6,1]
["6AG41312DB222AX6","SIMATIC IPC627D (BOX PC), HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; CORE I3-4330TE (2C/4T, 2.4GHZ, 4MB CACHE, VT-X); 250 GB HDD SATA; DVD+/-RW; 4 GB DDR3 1600 DIMM; 1 X PCIE (X16); 1 X PCIE (X4); COM2; LPT (1 SLOT OCCUPIED); WINDOWS 7 ULTIMATE 32BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); DC 24V  INDUSTRAL- POWER SUPPLY;",2957,"TEM",1,"Simatic",6,1]
["6AG41312DB222BX6","SIMATIC IPC627D (BOX PC), HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; CORE I3-4330TE (2C/4T, 2.4GHZ, 4MB CACHE, VT-X); 250 GB HDD SATA; DVD+/-RW; 4 GB DDR3 1600 DIMM; 1 X PCIE (X16); 1 X PCIE (X4); COM2; LPT (1 SLOT OCCUPIED); WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); DC 24V  INDUSTRAL- POWER SUPPLY;",2957,"TEM",1,"Simatic",6,1]
["6AG41312DB322BX6","SIMATIC IPC627D (BOX PC), HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; CORE I3-4330TE (2C/4T, 2.4GHZ, 4MB CACHE, VT-X); 250 GB HDD SATA; DVD+/-RW; 8 GB DDR3 1600 DIMM; 1 X PCIE (X16); 1 X PCIE (X4); COM2; LPT (1 SLOT OCCUPIED); WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); DC 24V  INDUSTRAL- POWER SUPPLY;",3104,"TEM",1,"Simatic",6,1]
["6AG41312DD210AX6","SIMATIC IPC627D (BOX PC), HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; CORE I3-4330TE (2C/4T, 2.4GHZ, 4MB CACHE, VT-X); 500 GB HDD SATA; 4 GB DDR3 1600 DIMM; 1 X PCIE (X16); 1 X  PCI; W/O EXTENSION (HW); WINDOWS 7 ULTIMATE 32BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); DC 24V  INDUSTRAL- POWER SUPPLY;",2810,"TEM",1,"Simatic",6,1]
["6AG41312DE500XX3","SIMATIC IPC627D (BOX PC), HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; CORE I3-4330TE (2C/4T, 2.4GHZ, 4MB CACHE, VT-X); 500 GB HDD SATA; DVD+/-RW; 8 GB DDR3 1600 DIMM; ECC; 2 X  PCI; W/O EXTENSION (HW); W/O OPERATING SYSTEM; W/O  EXTENSION (SW); AC 110/230V INDUSTRIAL POWER SUPPLY WITH NAMUR; POWER CORD USA;",2926,"TEM",1,"Simatic",6,1]
["6AG41312DM310BX3","SIMATIC IPC627D (BOX PC), HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; CORE I3-4330TE (2C/4T, 2.4GHZ, 4MB CACHE, VT-X); SOLID STATE DRIVE 240 GB; 8 GB DDR3 1600 DIMM; 1 X PCIE (X16); 1 X  PCI; W/O EXTENSION (HW); WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); AC 110/230V INDUSTRIAL POWER SUPPLY WITH NAMUR; POWER CORD USA;",3251,"TEM",1,"Simatic",6,1]
["6AG41312DM311BC3","SIMATIC IPC627D (BOX PC), HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; CORE I3-4330TE (2C/4T, 2.4GHZ, 4MB CACHE, VT-X); SOLID STATE DRIVE 240 GB; 8 GB DDR3 1600 DIMM; 1 X PCIE (X16); 1 X  PCI; 2X USB ADDITIV 1 SLOT OCCUPIED; WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); SIMATIC IPC DIAGMONITOR V4.5 & IMAGE&PARTITION CREATOR V3.4 ADDED; AC 110/230V INDUSTRIAL POWER SUPPLY WITH NAMUR; POWER CORD USA;",3535,"TEM",1,"Simatic",6,1]
["6AG41312FP413BC3","SIMATIC IPC627D (BOX PC), HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; CORE I3-4330TE (2C/4T, 2.4GHZ, 4MB CACHE, VT-X); PROFINET (IRT, 3 PORTS, CP1616-COMPATIBLE); 2 MB BUFFERED SRAM; SOLID STATE DRIVE 240 GB; 320 GB HDD SATA (2,5\"); DVD+/-RW; 16 GB DDR3 1600 DIMM; 1 X PCIE (X16); 1 X  PCI; 2X USB ADDITIV; COM2; LPT (2 SLOTS OCCUPIED); WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); SIMATIC IPC DIAGMONITOR V4.5 & IMAGE&PARTITION CREATOR V3.4 ADDED; AC 110/230V INDUSTRIAL POWER SUPPLY WITH NAMUR; POWER CORD USA;",4952,"TEM",1,"Simatic",6,1]
["6AG41312GH200AX3","SIMATIC IPC627D (BOX PC), HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; XEON E3-1268LV3 (4C/8T, 2,3(3.3)GHZ, 8MB CACHE VT-D, AMT); RAID1 2 X 320 GB SATA (2,5\"); DVD+/-RW; 4 GB DDR3 1600 DIMM; 2 X  PCI; W/O EXTENSION (HW); WINDOWS 7 ULTIMATE 32BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); AC 110/230V INDUSTRIAL POWER SUPPLY WITH NAMUR; POWER CORD USA;",3766,"TEM",1,"Simatic",6,1]
["6AG41312GM220AX6","SIMATIC IPC627D (BOX PC), HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; XEON E3-1268LV3 (4C/8T, 2,3(3.3)GHZ, 8MB CACHE VT-D, AMT); SOLID STATE DRIVE 240 GB; 4 GB DDR3 1600 DIMM; 1 X PCIE (X16); 1 X PCIE (X4); W/O EXTENSION (HW); WINDOWS 7 ULTIMATE 32BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); DC 24V  INDUSTRAL- POWER SUPPLY;",3535,"TEM",1,"Simatic",6,1]
["6AG41312GM320BX3","SIMATIC IPC627D (BOX PC), HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; XEON E3-1268LV3 (4C/8T, 2,3(3.3)GHZ, 8MB CACHE VT-D, AMT); SOLID STATE DRIVE 240 GB; 8 GB DDR3 1600 DIMM; 1 X PCIE (X16); 1 X PCIE (X4); W/O EXTENSION (HW); WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); AC 110/230V INDUSTRIAL POWER SUPPLY WITH NAMUR; POWER CORD USA;",3682,"TEM",1,"Simatic",6,1]
["6AG41312GM413BX6","SIMATIC IPC627D (BOX PC), HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; XEON E3-1268LV3 (4C/8T, 2,3(3.3)GHZ, 8MB CACHE VT-D, AMT); SOLID STATE DRIVE 240 GB; 16 GB DDR3 1600 DIMM; 1 X PCIE (X16); 1 X  PCI; 2X USB ADDITIV; COM2; LPT (2 SLOTS OCCUPIED); WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); DC 24V  INDUSTRAL- POWER SUPPLY;",4144,"TEM",1,"Simatic",6,1]
["6AG41312GN600BA6","SIMATIC IPC627D (BOX PC), HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; XEON E3-1268LV3 (4C/8T, 2,3(3.3)GHZ, 8MB CACHE VT-D, AMT); SOLID STATE DRIVE 240 GB; 320 GB HDD SATA (2,5\"); 16 GB DDR3 1600 DIMM; ECC; 2 X  PCI; W/O EXTENSION (HW); WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); SIMATIC IPC DIAGMONITOR V4.5 ADDED; DC 24V  INDUSTRAL- POWER SUPPLY;",4616,"TEM",1,"Simatic",6,1]
["6AG41312GP200BX0","SIMATIC IPC627D (BOX PC), HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; XEON E3-1268LV3 (4C/8T, 2,3(3.3)GHZ, 8MB CACHE VT-D, AMT); SOLID STATE DRIVE 240 GB; 320 GB HDD SATA (2,5\"); DVD+/-RW; 4 GB DDR3 1600 DIMM; 2 X  PCI; W/O EXTENSION (HW); WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); AC 110/230V INDUSTRIAL POWER SUPPLY WITH NAMUR; POWER CORD EUROPE;",3871,"TEM",1,"Simatic",6,1]
["6AG41312HM312BX0","SIMATIC IPC627D (BOX PC), HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; XEON E3-1268LV3 (4C/8T, 2.3(3.3)GHZ, 8MB CACHE VT-D, AMT); PROFIBUS/MPI CP5622-COMPATIBLE); 2 MB BUFFERED SRAM; SOLID STATE DRIVE 240 GB; 8 GB DDR3 1600 DIMM; 1 X PCIE (X16); 1 X  PCI; COM2; LPT (1 SLOT OCCUPIED); WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); AC 110/230V INDUSTRIAL POWER SUPPLY WITH NAMUR; POWER CORD EUROPE;",3955,"TEM",1,"Simatic",6,1]
["6AG41312JH411BX3","SIMATIC IPC627D (BOX PC), HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; XEON E3-1268LV3 (4C/8T, 2.3(3.3)GHZ, 8MB CACHE VT-D, AMT); PROFINET (IRT, 3 PORTS, CP1616-COMPATIBLE); 2 MB BUFFERED SRAM; RAID1 2 X 320 GB SATA (2,5\"); DVD+/-RW; 16 GB DDR3 1600 DIMM; 1 X PCIE (X16); 1 X  PCI; 2X USB ADDITIV 1 SLOT OCCUPIED; WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); AC 110/230V INDUSTRIAL POWER SUPPLY WITH NAMUR; POWER CORD USA;",4994,"TEM",1,"Simatic",6,1]
["6AG41312JH610AA3","SIMATIC IPC627D (BOX PC), HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; XEON E3-1268LV3 (4C/8T, 2.3(3.3)GHZ, 8MB CACHE VT-D, AMT); PROFINET (IRT, 3 PORTS, CP1616-COMPATIBLE); 2 MB BUFFERED SRAM; RAID1 2 X 320 GB SATA (2,5\"); DVD+/-RW; 16 GB DDR3 1600 DIMM; ECC; 1 X PCIE (X16); 1 X  PCI; W/O EXTENSION (HW); WINDOWS 7 ULTIMATE 32BIT SP1, MUI (EN, GE, FR, IT, SP); SIMATIC IPC DIAGMONITOR V4.5 ADDED; AC 110/230V INDUSTRIAL POWER SUPPLY WITH NAMUR; POWER CORD USA;",5393,"TEM",1,"Simatic",6,1]
["6AG41322GE400BX3","SIMATIC IPC827D (BOX PC) HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; XEON E3-1268LV3 4C/8T, 2,3(3.3)GHZ, 8MB CACHE VT-D, AMT); 500 GB HDD SATA; DVD+/-RW; 16 GB DDR3 1600 DIMM; 1 X PCIE (X16); 1 X PCIE (X4); 3 X PCI; W/O EXTENSION (HW); WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); AC 110/230V INDUSTRIAL POWER SUPPLY WITH NAMUR; POWER CORD USA;",4064,"TEM",1,"Simatic",6,1]
["6AG41322GG600BA6","SIMATIC IPC827D (BOX PC) HD GRAPHIC ONBOARD, 2 X GIGABIT ETHERNET (IE/PN) 4 X USB V3.0; 1 X SERIELL (COM1); RAID-CONTROLLER ON BOARD; WATCHDOG, STP.-/FAN- MONITORING; XEON E3-1268LV3 4C/8T, 2,3(3.3)GHZ, 8MB CACHE VT-D, AMT); RAID1 2 X 320 GB SATA (2,5\"); 16 GB DDR3 1600 DIMM; ECC; 1 X PCIE (X16); 1 X PCIE (X4); 3 X PCI; W/O EXTENSION (HW); WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); SIMATIC IPC DIAGMONITOR V4.5 ADDED; DC 24V  INDUSTRAL- POWER SUPPLY;",4725,"TEM",1,"Simatic",6,1]
["6AG41400BA000CA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 1 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: W/O OPERATING SYSTEM; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: CFAST 4 GB, W/O SIMATIC SOFTWARE;",1305,"TEM",1,"Simatic",3,1]
["6AG41400BB000HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: W/O OPERATING SYSTEM; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",1504,"TEM",1,"Simatic",3,1]
["6AG41400BB040CA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: CFAST 4 GB, W/O SIMATIC SOFTWARE;",1494,"TEM",1,"Simatic",3,1]
["6AG41400BB042CC0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: CFAST 4 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: CFAST 4 GB, WIN CC RT ADV. V13 SP1 128PT (INCL. LOGGING AND RECIPES);",1914,"TEM",1,"Simatic",3,1]
["6AG41400BB043AA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: CFAST 8 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: W/O MASS STORAGE INTERNAL; W/O SIMATIC SOFTWARE;",1609,"TEM",1,"Simatic",3,1]
["6AG41400BB070HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",1840,"TEM",1,"Simatic",3,1]
["6AG41400BB140HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",1767,"TEM",1,"Simatic",3,1]
["6AG41400BB360KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 2 GB; EXTENSION (HW): 2X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",1824,"TEM",1,"Simatic",3,1]
["6AG41400BC043AA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: CFAST 8 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: W/O MASS STORAGE INTERNAL; W/O SIMATIC SOFTWARE;",1693,"TEM",1,"Simatic",3,1]
["6AG41400BC060KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",1830,"TEM",1,"Simatic",3,1]
["6AG41400BC070HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",1924,"TEM",1,"Simatic",3,1]
["6AG41400BC370KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 2X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",1908,"TEM",1,"Simatic",3,1]
["6AG41400BK040HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 2 GB WITH NVRAM; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",1714,"TEM",1,"Simatic",3,1]
["6AG41400BL040HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB WITH NVRAM; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",1798,"TEM",1,"Simatic",3,1]
["6AG41400BL060HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB WITH NVRAM; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",1977,"TEM",1,"Simatic",3,1]
["6AG41400DC042KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: CFAST 4 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",1788,"TEM",1,"Simatic",3,1]
["6AG41401BC170KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2145,"TEM",1,"Simatic",3,1]
["6AG41401BL573HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB WITH NVRAM; EXTENSION (HW): 2X RS232; 2X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: CFAST 8 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2727,"TEM",1,"Simatic",3,1]
["6AG41403BB000HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: W/O OPERATING SYSTEM; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",1861,"TEM",1,"Simatic",3,1]
["6AG41403BB040HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2019,"TEM",1,"Simatic",3,1]
["6AG41403BB060KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2103,"TEM",1,"Simatic",3,1]
["6AG41403BB070HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2197,"TEM",1,"Simatic",3,1]
["6AG41403BB070PA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2407,"TEM",1,"Simatic",3,1]
["6AG41403BB071HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: CFAST 2 GB, W/O SW; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2281,"TEM",1,"Simatic",3,1]
["6AG41403BB140HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2124,"TEM",1,"Simatic",3,1]
["6AG41403BB170KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2208,"TEM",1,"Simatic",3,1]
["6AG41403BB360KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 2 GB; EXTENSION (HW): 2X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2181,"TEM",1,"Simatic",3,1]
["6AG41403BC060KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2187,"TEM",1,"Simatic",3,1]
["6AG41403BC070HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2281,"TEM",1,"Simatic",3,1]
["6AG41403BC070KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2187,"TEM",1,"Simatic",3,1]
["6AG41403BC070KA8","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; WITH TPM, *NOT FOR CHINA AND RUSSIA* PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2240,"TEM",1,"Simatic",3,1]
["6AG41403BC072HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: CFAST 4 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2418,"TEM",1,"Simatic",3,1]
["6AG41403BC072PA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: CFAST 4 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2628,"TEM",1,"Simatic",3,1]
["6AG41403BC163KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 32BIT; MASS STORAGE CHANGEABLE: CFAST 8 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2544,"TEM",1,"Simatic",3,1]
["6AG41403BC170KA8","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; WITH TPM, *NOT FOR CHINA AND RUSSIA* PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2345,"TEM",1,"Simatic",3,1]
["6AG41403BC370KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 2X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2265,"TEM",1,"Simatic",3,1]
["6AG41403BD070HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2428,"TEM",1,"Simatic",3,1]
["6AG41403BD070PA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2638,"TEM",1,"Simatic",3,1]
["6AG41403BD150KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7 SP1, ENGLISH, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2260,"TEM",1,"Simatic",3,1]
["6AG41403BL140HJ0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB WITH NVRAM; EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); WINAC RTX 2010 SP2; WIN CC RT ADV. V13 SP1 128PT (INCL. LOGGING AND RECIPES);",3310,"TEM",1,"Simatic",3,1]
["6AG41403BM370HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB WITH NVRAM; EXTENSION (HW): 2X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2559,"TEM",1,"Simatic",3,1]
["6AG41403BM370KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB WITH NVRAM; EXTENSION (HW): 2X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2465,"TEM",1,"Simatic",3,1]
["6AG41403DA040KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 1 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",1893,"TEM",1,"Simatic",3,1]
["6AG41403DB000HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: W/O OPERATING SYSTEM; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",1861,"TEM",1,"Simatic",3,1]
["6AG41403DB060HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2197,"TEM",1,"Simatic",3,1]
["6AG41403DC040CA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: CFAST 4 GB, W/O SIMATIC SOFTWARE;",1935,"TEM",1,"Simatic",3,1]
["6AG41403DC040HC0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); WIN CC RT ADV. V13 SP1 128PT (INCL. LOGGING AND RECIPES);",2386,"TEM",1,"Simatic",3,1]
["6AG41403DC040PD0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); WIN CC RT ADV. V13 SP1 512PT (INCL. LOGGING AND RECIPES);",3205,"TEM",1,"Simatic",3,1]
["6AG41403DC051HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7 SP1, ENGLISH, 64BIT; MASS STORAGE CHANGEABLE: CFAST 2 GB, W/O SW; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2187,"TEM",1,"Simatic",3,1]
["6AG41403DC070HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2281,"TEM",1,"Simatic",3,1]
["6AG41403DC140CA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: CFAST 4 GB, W/O SIMATIC SOFTWARE;",2040,"TEM",1,"Simatic",3,1]
["6AG41403DC270HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; 2X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2491,"TEM",1,"Simatic",3,1]
["6AG41403DC370KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 2X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2265,"TEM",1,"Simatic",3,1]
["6AG41403DC541KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 2X RS232; 2X PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: CFAST 2 GB, W/O SW; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2381,"TEM",1,"Simatic",3,1]
["6AG41403DD070HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2428,"TEM",1,"Simatic",3,1]
["6AG41403DD340HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 2X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2328,"TEM",1,"Simatic",3,1]
["6AG41403DD370KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 2X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2412,"TEM",1,"Simatic",3,1]
["6AG41403EC070HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: BOOK MOUNTING; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2281,"TEM",1,"Simatic",3,1]
["6AG41403EC541CA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: BOOK MOUNTING; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 2X RS232; 2X PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: CFAST 2 GB, W/O SW; MASS STORAGE INTERNAL: CFAST 4 GB, W/O SIMATIC SOFTWARE;",2307,"TEM",1,"Simatic",3,1]
["6AG41404BB362HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 2 GB; EXTENSION (HW): 2X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 32BIT; MASS STORAGE CHANGEABLE: CFAST 4 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2622,"TEM",1,"Simatic",3,1]
["6AG41404BC040DA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: CFAST 8 GB, W/O SIMATIC SOFTWARE;",2260,"TEM",1,"Simatic",3,1]
["6AG41404BC043AA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: CFAST 8 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: W/O MASS STORAGE INTERNAL; W/O SIMATIC SOFTWARE;",2260,"TEM",1,"Simatic",3,1]
["6AG41404BC362HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 2X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 32BIT; MASS STORAGE CHANGEABLE: CFAST 4 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2706,"TEM",1,"Simatic",3,1]
["6AG41404BC362KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 2X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 32BIT; MASS STORAGE CHANGEABLE: CFAST 4 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2612,"TEM",1,"Simatic",3,1]
["6AG41404BD240HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; 2X PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2670,"TEM",1,"Simatic",3,1]
["6AG41404BL044AA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB WITH NVRAM; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: CFAST 16 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: W/O MASS STORAGE INTERNAL; W/O SIMATIC SOFTWARE;",2470,"TEM",1,"Simatic",3,1]
["6AG41404DC170KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2502,"TEM",1,"Simatic",3,1]
["6AG41405BD170KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I3-3217UE; 1 X GBIT ETHERNET (IE/PN); 1 X PROFINET (IRT, 3 PORTS); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",3048,"TEM",1,"Simatic",3,1]
["6AG41406BB140HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2386,"TEM",1,"Simatic",3,1]
["6AG41406BB201AA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; 2X PCIE; OPERATING SYSTEM: W/O OPERATING SYSTEM; MASS STORAGE CHANGEABLE: CFAST 2 GB, W/O SW; MASS STORAGE INTERNAL: W/O MASS STORAGE INTERNAL; W/O SIMATIC SOFTWARE;",2113,"TEM",1,"Simatic",3,1]
["6AG41406BC000HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: W/O OPERATING SYSTEM; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2208,"TEM",1,"Simatic",3,1]
["6AG41406BC040HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2365,"TEM",1,"Simatic",3,1]
["6AG41406BC070HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2544,"TEM",1,"Simatic",3,1]
["6AG41406BC070KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2449,"TEM",1,"Simatic",3,1]
["6AG41406BC170PA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2859,"TEM",1,"Simatic",3,1]
["6AG41406BC172PA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: CFAST 4 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2995,"TEM",1,"Simatic",3,1]
["6AG41406BC470HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 2X RS232; 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2727,"TEM",1,"Simatic",3,1]
["6AG41406BC471KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 2X RS232; 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: CFAST 2 GB, W/O SW; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2717,"TEM",1,"Simatic",3,1]
["6AG41406BD050HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7 SP1, ENGLISH, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2512,"TEM",1,"Simatic",3,1]
["6AG41406BD070HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2691,"TEM",1,"Simatic",3,1]
["6AG41406BD070KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2596,"TEM",1,"Simatic",3,1]
["6AG41406BD070PA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2901,"TEM",1,"Simatic",3,1]
["6AG41406BD100HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: W/O OPERATING SYSTEM; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2460,"TEM",1,"Simatic",3,1]
["6AG41406BD170HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2796,"TEM",1,"Simatic",3,1]
["6AG41406BD170PA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",3006,"TEM",1,"Simatic",3.081,1]
["6AG41406BD200HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; 2X PCIE; OPERATING SYSTEM: W/O OPERATING SYSTEM; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2565,"TEM",1,"Simatic",3,1]
["6AG41406BD200PA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; 2X PCIE; OPERATING SYSTEM: W/O OPERATING SYSTEM; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2775,"TEM",1,"Simatic",3,1]
["6AG41406BD354HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 2X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7 SP1, ENGLISH, 64BIT; MASS STORAGE CHANGEABLE: CFAST 16 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",3000,"TEM",1,"Simatic",3,1]
["6AG41406BG060HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB WITH ECC; (ONLY WITH CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN)); EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2575,"TEM",1,"Simatic",3,1]
["6AG41406BG201AA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB WITH ECC; (ONLY WITH CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN)); EXTENSION (HW): 1X RS232; 2X PCIE; OPERATING SYSTEM: W/O OPERATING SYSTEM; MASS STORAGE CHANGEABLE: CFAST 2 GB, W/O SW; MASS STORAGE INTERNAL: W/O MASS STORAGE INTERNAL; W/O SIMATIC SOFTWARE;",2229,"TEM",1,"Simatic",3,1]
["6AG41406BH070KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB MIT ECC; (ONLY WITH CORE I7-3517UE); EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2775,"TEM",1,"Simatic",3,1]
["6AG41406BH254HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB MIT ECC; (ONLY WITH CORE I7-3517UE); EXTENSION (HW): 1X RS232; 2X PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7 SP1, ENGLISH, 64BIT; MASS STORAGE CHANGEABLE: CFAST 16 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",3310,"TEM",1,"Simatic",3,1]
["6AG41406BH270HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB MIT ECC; (ONLY WITH CORE I7-3517UE); EXTENSION (HW): 1X RS232; 2X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",3079,"TEM",1,"Simatic",3,1]
["6AG41406BM040HB0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB WITH NVRAM; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); WINAC RTX 2010 SP2;",3331,"TEM",1,"Simatic",3,1]
["6AG41406BM070HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB WITH NVRAM; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2743,"TEM",1,"Simatic",3,1]
["6AG41406BM542PC0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB WITH NVRAM; EXTENSION (HW): 2X RS232; 2X PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: CFAST 4 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); WIN CC RT ADV. V13 SP1 128PT (INCL. LOGGING AND RECIPES);",3483,"TEM",1,"Simatic",3,1]
["6AG41406BP170PA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB WITH ECC AND NVRAM; (ONLY WITH CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN)); EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",3237,"TEM",1,"Simatic",3,1]
["6AG41406BP473HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB WITH ECC AND NVRAM; (ONLY WITH CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN)); EXTENSION (HW): 2X RS232; 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: CFAST 8 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",3357,"TEM",1,"Simatic",3,1]
["6AG41406BP560KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB WITH ECC AND NVRAM; (ONLY WITH CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN)); EXTENSION (HW): 2X RS232; 2X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",3116,"TEM",1,"Simatic",3,1]
["6AG41406DC040CA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: CFAST 4 GB, W/O SIMATIC SOFTWARE;",2197,"TEM",1,"Simatic",3,1]
["6AG41406DC362KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 2X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 32BIT; MASS STORAGE CHANGEABLE: CFAST 4 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2664,"TEM",1,"Simatic",3,1]
["6AG41406DC370KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 2X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2528,"TEM",1,"Simatic",3,1]
["6AG41406DD070KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2596,"TEM",1,"Simatic",3,1]
["6AG41406DD070PA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2901,"TEM",1,"Simatic",3,1]
["6AG41406DD170PA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",3006,"TEM",1,"Simatic",3,1]
["6AG41406DD370KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 2X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2675,"TEM",1,"Simatic",3,1]
["6AG41406DH070PA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 8 GB MIT ECC; (ONLY WITH CORE I7-3517UE); EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",3079,"TEM",1,"Simatic",3,1]
["6AG41406DH244HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 8 GB MIT ECC; (ONLY WITH CORE I7-3517UE); EXTENSION (HW): 1X RS232; 2X PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: CFAST 16 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",3310,"TEM",1,"Simatic",3,1]
["6AG41406DH270HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 8 GB MIT ECC; (ONLY WITH CORE I7-3517UE); EXTENSION (HW): 1X RS232; 2X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",3079,"TEM",1,"Simatic",3,1]
["6AG41406DN170HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 4 GB WITH ECC AND NVRAM; (ONLY WITH CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN)); EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2733,"TEM",1,"Simatic",3,1]
["6AG41406DP073HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 8 GB WITH ECC AND NVRAM; (ONLY WITH CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN)); EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: CFAST 8 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",3174,"TEM",1,"Simatic",3,1]
["6AG41406EC270KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: BOOK MOUNTING; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; 2X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2659,"TEM",1,"Simatic",3,1]
["6AG41406ED170AK0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: BOOK MOUNTING; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: W/O MASS STORAGE INTERNAL; WINAC RTX 2010 SP2; WIN CC RT ADV. V13 SP1 512PT (INCL. LOGGING AND RECIPES);",4150,"TEM",1,"Simatic",3,1]
["6AG41406ED170KA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MOUNTING: BOOK MOUNTING; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE;",2701,"TEM",1,"Simatic",3,1]
["6AG41407BC170HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2859,"TEM",1,"Simatic",3,1]
["6AG41407BD570PA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 2X RS232; 2X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",3399,"TEM",1,"Simatic",3,1]
["6AG41407BL060PA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB WITH NVRAM; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",3016,"TEM",1,"Simatic",3,1]
["6AG41407DD274HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; 2X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: CFAST 16 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",3520,"TEM",1,"Simatic",3,1]
["6AG41407DL040HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 4 GB WITH NVRAM; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",2628,"TEM",1,"Simatic",3,1]
["6AG41407EL143AN0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MOUNTING: BOOK MOUNTING; MEMORY EXTENSION: 4 GB WITH NVRAM; EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: CFAST 8 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: W/O MASS STORAGE INTERNAL; WINAC RTX F 2010 SP2;",3762,"TEM",1,"Simatic",3,1]
["6AG41408BD170HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 1 X GBIT ETHERNET (IE/PN); 1 X PROFINET (IRT, 3 PORTS); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",3405,"TEM",1,"Simatic",3,1]
["6AG41408BL042HK0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 1 X GBIT ETHERNET (IE/PN); 1 X PROFINET (IRT, 3 PORTS); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB WITH NVRAM; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: CFAST 4 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); WINAC RTX 2010 SP2; WIN CC RT ADV. V13 SP1 512PT (INCL. LOGGING AND RECIPES);",4822,"TEM",1,"Simatic",3,1]
["6AG41408BL042HP0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 1 X GBIT ETHERNET (IE/PN); 1 X PROFINET (IRT, 3 PORTS); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 4 GB WITH NVRAM; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: CFAST 4 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); WINAC RTX F 2010 SP2; WIN CC RT ADV. V13 SP1 128PT (INCL. LOGGING AND RECIPES);",4528,"TEM",1,"Simatic",3,1]
["6AG41408BM041HB0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 1 X GBIT ETHERNET (IE/PN); 1 X PROFINET (IRT, 3 PORTS); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB WITH NVRAM; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: CFAST 2 GB, W/O SW; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); WINAC RTX 2010 SP2;",4024,"TEM",1,"Simatic",3,1]
["6AG41408BM163HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 1 X GBIT ETHERNET (IE/PN); 1 X PROFINET (IRT, 3 PORTS); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB WITH NVRAM; EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 32BIT; MASS STORAGE CHANGEABLE: CFAST 8 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",3709,"TEM",1,"Simatic",3,1]
["6AG41408BM344PA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 1 X GBIT ETHERNET (IE/PN); 1 X PROFINET (IRT, 3 PORTS); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB WITH NVRAM; EXTENSION (HW): 2X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: CFAST 16 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",3872,"TEM",1,"Simatic",3,1]
["6AG41408BM500PA8","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; WITH TPM, *NOT FOR CHINA AND RUSSIA* PROCESSOR: CORE I7-3517UE; 1 X GBIT ETHERNET (IE/PN); 1 X PROFINET (IRT, 3 PORTS); MOUNTING ACCESSORIES: MOUNTING ON DIN RAIL; MEMORY EXTENSION: 8 GB WITH NVRAM; EXTENSION (HW): 2X RS232; 2X PCIE; OPERATING SYSTEM: W/O OPERATING SYSTEM; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",3568,"TEM",1,"Simatic",3,1]
["6AG41408DL141HA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 1 X GBIT ETHERNET (IE/PN); 1 X PROFINET (IRT, 3 PORTS); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 4 GB WITH NVRAM; EXTENSION (HW): 1X RS232; 1X PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: CFAST 2 GB, W/O SW; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",3216,"TEM",1,"Simatic",3,1]
["6AG41408DM040PA0","SIMATIC IPC427D (MICROBOX PC), HD GRAPHIC ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45, 4 X USB V3.0 (HIGH CURRENT), PCIE (OPTIONAL), 24V DC POWER SUPPLY; PROCESSOR: CORE I7-3517UE; 1 X GBIT ETHERNET (IE/PN); 1 X PROFINET (IRT, 3 PORTS); MOUNTING: WALL MOUNTING; MEMORY EXTENSION: 8 GB WITH NVRAM; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",3384,"TEM",1,"Simatic",3,1]
["6AV21446QB040AS0","VW EF /38/VN54X/FT OPERATOR STATION, SIMATIC HMI TP1500, BASIC PANEL, TOUCH, 15\" WIDESCREEN, TFT-DISPLAY, SCALANCE X202 3SB OPERATING COMPONENTS, SIGNAL LIGHT RED, YELLOW VN54X CRAFTER WRZESNIA",6782,"TEM",1,"Simatic",60,0]
["6AV21446QE030AS0","AU FT/22/AU651/FT_MO NECKARSULM OPERATOR STATION, SIMATIC HMI TP1500, COMFORT PANEL, , TOUCH, 15\" WIDESCREEN, TFT-DISPLAY, WINDOWS CE 6.0, SD CARD 2GB, SIMATIC ET 200SP IM155-6PN, 3SB OPERATING COMPONENTS, SIGNAL LIGHT RED",6143,"TEM",1,"Simatic",50,0]
["6AV21446QE031AS0","AU FT/46/AU516/FT_MO BrÃ¼ssel operator STation, SIMATIC HMI TP1500, Comfort Panel, Touch, 15\" widescreen, TFT display, Windows CE 6.0, SD card 2 GB, SIMATIC ET 200SP IM155-6PN, 3SU operating components, signal light red",6143,"TEM",1,"Simatic",55,0]
["6AV36884AY000AS1","OPERATOR STAT. OEM SGBB VW KP8, ET200S, SCALANCE X202 VW SGBB/SAG/E22/ROW",2985,"TEM",1,"Simatic",10,0]
["6AV36884AY000AS3","OPERATOR STAT. OEM SGBB VW/AUDI VW SG-BEDIENBOX/SAG/E22/RDW KP8, ET200S, SCALANCE X202",2953,"TEM",1,"Simatic",1E-3,0]
["6AV36884AY000PE0","OPERATOR STAT. OEM SGBB PORSCHE KP8, ET200S, SCALANCE X202 PORSCHE SGBB/SAG/MS20/RDW PORSCHE PO 416 MACAN, PORSCHE PO 623 PANAMERA LEIPZIG",3715,"TEM",1,"Simatic",10,0]
["6AV36884AY010AS1","OPERATOR STAT. OEM SGBB VW KP8, ET200S, SCALANCE X202 VW SGBB/SAG/E2/ROW NEW",2985,"TEM",1,"Simatic",10,0]
["6AV36884AY010AS2","VW SGBB/SAG/E2/NAR/UL OPERATOR STAT. OEM SGBB VW KP8, ET200S, SCALANCE X202",3128,"TEM",1,"Simatic",10,0]
["6AV36884AY010AS3","OPERATOR STAT. OEM SGBB VW/AUDI VW SG-BEDIENBOX/SAG/E2/RDW KP8, ET200S, SCALANCE X202",2953,"TEM",1,"Simatic",10,0]
["6AV36885BA210BK0","INTEGRA HVO 45/55 PROFINET, HOUSING WITH SIMATIC KP8",1005,"TEM",1,"Simatic",5,0]
["6AV36885CA160BK0","DAIMLER IW5, HVO 50, PROFINET, CASE RAL7035, SIMATIC HMI KP32F PN, EMERGENCY STOP, DIV. 3SB3 ELEMENTS",2287,"TEM",1,"Simatic",10,0]
["6AV36885CA760BK0","DAIMLER IW5, HVO 52, PROFINET SIMATIC IFP1500 MT, SIMATIC IPC227E, CELERON N2807 (2C/2T), 2GB RAM, 80 GB SOLID-STATE DRIVE SATA, WINDOWS 7 ULTIMATE SP1, 32BIT, SIMATIC HMI KP32F PN, EMERGENCY STOP, DIF. 3SB3 ELEMENTS, IMAGE INTEGRA HVO52",6869,"TEM",1,"Simatic",26,0]
["6AV66461AA220AX0","SIMATIC ITC1200, INDUSTRIAL THIN CLIENT, 12\" WIDESCREEN-TFT-DISPLAY, TOUCH OPERATION, SUPPORTED PROTOCOLS: RDP, VNC, SMARTSERVER, WEB",1208,"TEM",1,"Simatic",4.4800000000000004,1]
["6AV66461AB220AX0","SIMATIC ITC1500, INDUSTRIAL THIN CLIENT, 15\" WIDESCREEN-TFT-DISPLAY, TOUCH OPERATION, SUPPORTED PROTOCOLS: RDP, VNC, SMARTSERVER, WEB",1418,"TEM",1,"Simatic",7.2,1]
["6AV66461AC220AX0","SIMATIC ITC1900, INDUSTRIAL THIN CLIENT, 19\" WIDESCREEN-TFT-DISPLAY, TOUCH OPERATION, SUPPORTED PROTOCOLS: RDP, VNC, SMARTSERVER, WEB",1628,"TEM",1,"Simatic",8.5,1]
["6AV66461AD220AX0","SIMATIC ITC2200, INDUSTRIAL THIN CLIENT, 22\" WIDESCREEN-TFT-DISPLAY, TOUCH OPERATION, SUPPORTED PROTOCOLS: RDP, VNC, SMARTSERVER, WEB",2048,"TEM",1,"Simatic",9.1999999999999993,1]
["6AV66462AB212AX0","SIMATIC THIN CLIENT PROTECTED 15\" TOUCH,IP65, EXTERNAL DEVICE 15\" TFT DISPLAY, 64K COLORS, CLIENT: SMARTACCESS, RDP, WEB IP65 DEVICE FOR EXTERNAL MOUNTING, NO BUILT-IN UNIT",1554,"TEM",1,"Simatic",7.96,1]
["6AV72000AA000AA0","SIMATIC HMI THIN CLIENT EX 4X USB2.0, 2X RS232/422, POWER SUOOLY24V DC, TOUCH SCREEN WITH 8 F-KEYS ZONE 2: 15\"; NETWORK 10/100 BASE-TX, EX E; NO HOUSING; NO KEYBOARD;",6500,"TEM",1,"Simatic",19,0]
["6AV72000AA002AA0","SIMATIC HMI THIN CLIENT EX 4X USB2.0, 2X RS232/422, POWER SUOOLY24V DC, TOUCH SCREEN WITH 8 F-KEYS ZONE 2: 15\"; NETWORK 10/100 BASE-TX, EX E; INOX HOUSING; IP66, FOR WALL MOUNTING; NO KEYBOARD;",8449,"TEM",1,"Simatic",19,0]
["6AV72000EB006FA0","SIMATIC HMI THIN CLIENT EX 4X USB2.0, 2X RS232/422, POWER SUOOLY24V DC, TOUCH SCREEN WITH 8 F-KEYS ZONE 1: 19\"; NETWORK 100 BASE-FX FO (SC), EX OP IS; INOX HOUSING, IP66, FOR SWIVEL ARM INCL. TOP COUPLING, ROTATABLE 300 DEG ; KEYBOARD W. TRACKBALLQWERTY, MOUNTED IN KEYBOARD HOUSING;",13739,"TEM",1,"Simatic",19,0]
["6AV72400AA000AA8","SIMATIC IPC 477D WITH TPM, 12\" TOUCH DISPLAY; 4 USB (BACK) , ETHERNET (10/100/1000); 24V DC POWER SUPPLY, NOT FOR CHINA AND RUSSIA PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 1 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: W/O OPERATING SYSTEM; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: W/O MASS STORAGE INTERNAL; W/O SIMATIC SOFTWARE;",2163,"TEM",1,"Simatic",3.2,1]
["6AV72400AB040DA0","SIMATIC IPC 477D, 12\" TOUCH DISPLAY; 4 USB (BACK), ETHERNET (10/100/1000); PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: CFAST 8 GB; W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",2551,"TEM",1,"Simatic",3.2,1]
["6AV72400AB060HA0","SIMATIC IPC 477D, 12\" TOUCH DISPLAY; 4 USB (BACK), ETHERNET (10/100/1000); PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",2782,"TEM",1,"Simatic",3.2,1]
["6AV72400BB060HA3","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; AC 110/230V POWER SUPPLY WITH NAMUR; POWER CABLE FOR USA;",3023,"TEM",1,"Simatic",5,1]
["6AV72400BB360QA3","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 2 GB; EXTENSION (HW): 2X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; DVD; W/O SIMATIC SOFTWARE; AC 110/230V POWER SUPPLY WITH NAMUR; POWER CABLE FOR USA;",3207,"TEM",1,"Simatic",5,1]
["6AV72400BC070KA0","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",2981,"TEM",1,"Simatic",5,1]
["6AV72400BD370HA0","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 8 GB; EXTENSION (HW): 2X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3302,"TEM",1,"Simatic",5,1]
["6AV72400CB002KA0","SIMATIC IPC 477D, 15\" TOUCH/KEY DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: W/O OPERATING SYSTEM; MASS STORAGE CHANGEABLE: CFAST 4 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3065,"TEM",1,"Simatic",5.8,1]
["6AV72400CC060NA0","SIMATIC IPC 477D, 15\" TOUCH/KEY DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); DVD; W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3643,"TEM",1,"Simatic",5.8,1]
["6AV72400DA000AA0","SIMATIC IPC 477D, 19\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 1 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: W/O OPERATING SYSTEM; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: W/O MASS STORAGE INTERNAL; W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",2530,"TEM",1,"Simatic",6.4,1]
["6AV72400DC030KA0","SIMATIC IPC 477D, 19\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7 P SP1, ENGLISH, 32BIT, MULTITOUCH; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3160,"TEM",1,"Simatic",6.4,1]
["6AV72400DC070KA4","SIMATIC IPC 477D, 19\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE; AC 110/230V POWER SUPPLY WITH NAMUR; POWER CABLE FOR CHINA;",3223,"TEM",1,"Simatic",6.4,1]
["6AV72400DD070HA0","SIMATIC IPC 477D, 19\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3433,"TEM",1,"Simatic",6.4,1]
["6AV72400KK130QA3","SIMATIC IPC 477D, 19\" MULTITOUCH DISPLAY; 4USB (BACK); W/O USB (FRONT); ETHERNET (10/100/1000); PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 2 GB WITH NVRAM; EXTENSION (HW): 1X RS232 AND 1X PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7 P SP1, ENGLISH, 32BIT, MULTITOUCH; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; DVD; W/O SIMATIC SOFTWARE; AC 110/230V POWER SUPPLY WITH NAMUR; POWER CABLE FOR USA;",3674,"TEM",1,"Simatic",6.7,1]
["6AV72401AC342CA0","SIMATIC IPC 477D, 12\" TOUCH DISPLAY; 4 USB (BACK), ETHERNET (10/100/1000); PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 2X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: CFAST 4 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: CFAST 4 GB; W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",2945,"TEM",1,"Simatic",3.2,1]
["6AV72401AK042HA0","SIMATIC IPC 477D, 12\" TOUCH DISPLAY; 4 USB (BACK), ETHERNET (10/100/1000); PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MEMORY EXTENSION: 2 GB WITH NVRAM; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: CFAST 4 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3002,"TEM",1,"Simatic",3.2,1]
["6AV72401AK342HA0","SIMATIC IPC 477D, 12\" TOUCH DISPLAY; 4 USB (BACK), ETHERNET (10/100/1000); PROCESSOR: CELERON U827E; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MEMORY EXTENSION: 2 GB WITH NVRAM; EXTENSION (HW): 2X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: CFAST 4 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3081,"TEM",1,"Simatic",3.2,1]
["6AV72403AC040HA0","SIMATIC IPC 477D, 12\" TOUCH DISPLAY; 4 USB (BACK), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3044,"TEM",1,"Simatic",3.2,1]
["6AV72403AC070HA0","SIMATIC IPC 477D, 12\" TOUCH DISPLAY; 4 USB (BACK), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3223,"TEM",1,"Simatic",3.2,1]
["6AV72403BB040KA0","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3076,"TEM",1,"Simatic",5,1]
["6AV72403BB400PA0","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 2 GB; EXTENSION (HW): 2X RS232 AND 1X PCIE; OPERATING SYSTEM: W/O OPERATING SYSTEM; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3407,"TEM",1,"Simatic",5,1]
["6AV72403BC040HA0","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3254,"TEM",1,"Simatic",10,1]
["6AV72403BC070HA0","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3433,"TEM",1,"Simatic",5,1]
["6AV72403BC070KA3","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE; AC 110/230V POWER SUPPLY WITH NAMUR; POWER CABLE FOR USA;",3370,"TEM",1,"Simatic",5,1]
["6AV72403BD076PA3","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: DVD; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; AC 110/230V POWER SUPPLY WITH NAMUR; POWER CABLE FOR USA;",4021,"TEM",1,"Simatic",5,1]
["6AV72403CB440PA0","SIMATIC IPC 477D, 15\" TOUCH/KEY DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 2 GB; EXTENSION (HW): 2X RS232 AND 1X PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3932,"TEM",1,"Simatic",5.8,1]
["6AV72403CC070HA3","SIMATIC IPC 477D, 15\" TOUCH/KEY DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; AC 110/230V POWER SUPPLY WITH NAMUR; POWER CABLE FOR USA;",3832,"TEM",1,"Simatic",5.8,1]
["6AV72403DC040HA0","SIMATIC IPC 477D, 19\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3464,"TEM",1,"Simatic",6.4,1]
["6AV72403DC044CA0","SIMATIC IPC 477D, 19\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: CFAST 16 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: CFAST 4 GB; W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3706,"TEM",1,"Simatic",6.4,1]
["6AV72403DC066PA0","SIMATIC IPC 477D, 19\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 32BIT; MASS STORAGE CHANGEABLE: DVD; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",4052,"TEM",1,"Simatic",6.4,1]
["6AV72403DC070HA0","SIMATIC IPC 477D, 19\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3643,"TEM",1,"Simatic",6.4,1]
["6AV72403EC040HA0","SIMATIC IPC 477D, 22\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3884,"TEM",1,"Simatic",7,1]
["6AV72403EC040HA3","SIMATIC IPC 477D, 22\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; AC 110/230V POWER SUPPLY WITH NAMUR; POWER CABLE FOR USA;",3916,"TEM",1,"Simatic",7,1]
["6AV72403EC070HA0","SIMATIC IPC 477D, 22\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",4063,"TEM",1,"Simatic",7,1]
["6AV72403EC070KA3","SIMATIC IPC 477D, 22\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE; AC 110/230V POWER SUPPLY WITH NAMUR; POWER CABLE FOR USA;",4000,"TEM",1,"Simatic",7,1]
["6AV72404AC040DA0","SIMATIC IPC 477D, 12\" TOUCH DISPLAY; 4 USB (BACK), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: CFAST 8 GB; W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3202,"TEM",1,"Simatic",3.2,1]
["6AV72404AC040HE0","SIMATIC IPC 477D, 12\" TOUCH DISPLAY; 4 USB (BACK), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); WIN CC RT ADV. V13 SP1 2048PT (INCL. LOGGING AND RECIPES); DC24V INDUSTR. POWER SUPPLY; DC24V INDUSTR. POWER SUPPLY;",4625,"TEM",1,"Simatic",3.2,1]
["6AV72404BD060KA0","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3695,"TEM",1,"Simatic",5,1]
["6AV72404BK042HA0","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MEMORY EXTENSION: 2 GB WITH NVRAM; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: CFAST 4 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3569,"TEM",1,"Simatic",5,1]
["6AV72404BL372HA0","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MEMORY EXTENSION: 4 GB WITH NVRAM; EXTENSION (HW): 2X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: CFAST 4 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3911,"TEM",1,"Simatic",5,1]
["6AV72404DB043EC1","SIMATIC IPC 477D, 19\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: CFAST 8 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: CFAST 16 GB; WIN CC RT ADV. V13 SP1 128PT (INCL. LOGGING AND RECIPES); AC 110/230V POWER SUPPLY WITH NAMUR; W/O POWER CABLE;",4262,"TEM",1,"Simatic",6.4,1]
["6AV72404DL372HA0","SIMATIC IPC 477D, 19\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I3-3217UE; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MEMORY EXTENSION: 4 GB WITH NVRAM; EXTENSION (HW): 2X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: CFAST 4 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",4121,"TEM",1,"Simatic",6.4,1]
["6AV72406AD070PA0","SIMATIC IPC 477D, 12\" TOUCH DISPLAY; 4 USB (BACK), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3842,"TEM",1,"Simatic",3.2,1]
["6AV72406BA070KA0","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 1 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3485,"TEM",1,"Simatic",5,1]
["6AV72406BB070HA0","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3611,"TEM",1,"Simatic",5,1]
["6AV72406BC000HA0","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: W/O OPERATING SYSTEM; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3359,"TEM",1,"Simatic",5,1]
["6AV72406BC040HA1","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; AC 110/230V POWER SUPPLY WITH NAMUR; W/O POWER CABLE;",3548,"TEM",1,"Simatic",5,1]
["6AV72406BC070HA0","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3695,"TEM",1,"Simatic",5,1]
["6AV72406BC076PA0","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: DVD; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",4105,"TEM",1,"Simatic",5,1]
["6AV72406BD000HA0","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: W/O OPERATING SYSTEM; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3506,"TEM",1,"Simatic",5,1]
["6AV72406BD070KA0","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3748,"TEM",1,"Simatic",5,1]
["6AV72406BD170HA0","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232 AND 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3947,"TEM",1,"Simatic",5,1]
["6AV72406BD170KA0","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232 AND 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3853,"TEM",1,"Simatic",5,1]
["6AV72406BD170QA3","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232 AND 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; DVD; W/O SIMATIC SOFTWARE; AC 110/230V POWER SUPPLY WITH NAMUR; POWER CABLE FOR USA;",4084,"TEM",1,"Simatic",5,1]
["6AV72406BK040HJ3","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 2 GB WITH NVRAM; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); WINAC RTX 2010 SP2; WIN CC RT ADV. V13 SP1 128PT (INCL. LOGGING AND RECIPES); AC 110/230V POWER SUPPLY WITH NAMUR; POWER CABLE FOR USA;",4567,"TEM",1,"Simatic",5,1]
["6AV72406CB040HA0","SIMATIC IPC 477D, 15\" TOUCH/KEY DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 2 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3800,"TEM",1,"Simatic",5.8,1]
["6AV72406CB400PA0","SIMATIC IPC 477D, 15\" TOUCH/KEY DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 2 GB; EXTENSION (HW): 2X RS232 AND 1X PCIE; OPERATING SYSTEM: W/O OPERATING SYSTEM; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",4037,"TEM",1,"Simatic",5.8,1]
["6AV72406CB440PA0","SIMATIC IPC 477D, 15\" TOUCH/KEY DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 2 GB; EXTENSION (HW): 2X RS232 AND 1X PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",4194,"TEM",1,"Simatic",5.8,1]
["6AV72406CC066KA3","SIMATIC IPC 477D, 15\" TOUCH/KEY DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 32BIT; MASS STORAGE CHANGEABLE: DVD; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE; AC 110/230V POWER SUPPLY WITH NAMUR; POWER CABLE FOR USA;",4199,"TEM",1,"Simatic",5.8,1]
["6AV72406DC070HA0","SIMATIC IPC 477D, 19\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3905,"TEM",1,"Simatic",6.4,1]
["6AV72406DC070HA3","SIMATIC IPC 477D, 19\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; AC 110/230V POWER SUPPLY WITH NAMUR; POWER CABLE FOR USA;",3937,"TEM",1,"Simatic",6.4,1]
["6AV72406DC070KA0","SIMATIC IPC 477D, 19\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",3811,"TEM",1,"Simatic",6.4,1]
["6AV72406DC170NA3","SIMATIC IPC 477D, 19\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232 AND 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); DVD; W/O SIMATIC SOFTWARE; AC 110/230V POWER SUPPLY WITH NAMUR; POWER CABLE FOR USA;",4241,"TEM",1,"Simatic",6.4,1]
["6AV72406DC176HA3","SIMATIC IPC 477D, 19\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232 AND 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: DVD; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; AC 110/230V POWER SUPPLY WITH NAMUR; POWER CABLE FOR USA;",4241,"TEM",1,"Simatic",6.4,1]
["6AV72406DD070HA0","SIMATIC IPC 477D, 19\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY; DC24V INDUSTR. POWER SUPPLY;",4052,"TEM",1,"Simatic",6.4,1]
["6AV72406EC040HA0","SIMATIC IPC 477D, 22\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",4147,"TEM",1,"Simatic",7,1]
["6AV72406EC070HA0","SIMATIC IPC 477D, 22\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",4325,"TEM",1,"Simatic",7,1]
["6AV72406EC070NA0","SIMATIC IPC 477D, 22\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); DVD; W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",4525,"TEM",1,"Simatic",7,1]
["6AV72406EC170NA3","SIMATIC IPC 477D, 22\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232 AND 1X PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); DVD; W/O SIMATIC SOFTWARE; AC 110/230V POWER SUPPLY WITH NAMUR; POWER CABLE FOR USA;",4661,"TEM",1,"Simatic",7,1]
["6AV72406ED070HA0","SIMATIC IPC 477D, 22\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY; DC24V INDUSTR. POWER SUPPLY;",4472,"TEM",1,"Simatic",7,1]
["6AV72406ED070KA0","SIMATIC IPC 477D, 22\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: 320 GB HDD SATA; W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",4378,"TEM",1,"Simatic",7,1]
["6AV72406ED070PA0","SIMATIC IPC 477D, 22\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",4682,"TEM",1,"Simatic",7,1]
["6AV72406ED070PA3","SIMATIC IPC 477D, 22\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; AC 110/230V POWER SUPPLY WITH NAMUR; POWER CABLE FOR USA;",4714,"TEM",1,"Simatic",7,1]
["6AV72406ED076HA0","SIMATIC IPC 477D, 22\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: DVD; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",4672,"TEM",1,"Simatic",7,1]
["6AV72406EM372HA0","SIMATIC IPC 477D, 22\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 8 GB WITH NVRAM; EXTENSION (HW): 2X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: CFAST 4 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE; DC24V INDUSTR. POWER SUPPLY;",4740,"TEM",1,"Simatic",7,1]
["6AV72407BD044PF0","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MEMORY EXTENSION: 8 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: CFAST 16 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); WIN CC RT ADV. V13 SP1 4096PT (INCL. LOGGING AND RECIPES); DC24V INDUSTR. POWER SUPPLY;",6541,"TEM",1,"Simatic",5,1]
["6AV72407BM044PF0","SIMATIC IPC 477D, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 2 X GBIT ETHERNET (IE/PN); PROFIBUS DP 12; MEMORY EXTENSION: 8 GB WITH NVRAM; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN EMBEDDED STANDARD 7, 32BIT; MASS STORAGE CHANGEABLE: CFAST 16 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 240 GB STANDARD (MLC); WIN CC RT ADV. V13 SP1 4096PT (INCL. LOGGING AND RECIPES); DC24V INDUSTR. POWER SUPPLY;",6593,"TEM",1,"Simatic",5,1]
["6AV72408BC072HA8","SIMATIC IPC 477D WITH TPM, 15\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); 24V DC POWER SUPPLY, NOT FOR CHINA AND RUSSIA PROCESSOR: CORE I7-3517UE; 1 X GBIT ETHERNET (IE/PN);  1X PROFINET (IRT, 3 PORTS); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WINDOWS 7 ULTIMATE, 64BIT; MASS STORAGE CHANGEABLE: CFAST 4 GB, (ONLY WITH SW, IF NO INTERNAL MASS STORAGE); MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); W/O SIMATIC SOFTWARE;",4494,"TEM",1,"Simatic",5,1]
["6AV72408EM400NA3","SIMATIC IPC 477D, 22\" TOUCH DISPLAY; 4 USB (BACK) + 1 USB (FRONT), ETHERNET (10/100/1000); PROCESSOR: CORE I7-3517UE; 1 X GBIT ETHERNET (IE/PN);  1X PROFINET (IRT, 3 PORTS); MEMORY EXTENSION: 8 GB WITH NVRAM; EXTENSION (HW): 2X RS232 AND 1X PCIE; OPERATING SYSTEM: W/O OPERATING SYSTEM; MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB STANDARD (MLC); DVD; W/O SIMATIC SOFTWARE; AC 110/230V POWER SUPPLY WITH NAMUR; POWER CABLE FOR USA;",5213,"TEM",1,"Simatic",7,1]
["6AV72445AA101PT0","SIMATIC IPC 477D, 12\" TOUCH, MIT WINCC FLEX SW PACKAGE",4599,"TEM",1,"Simatic",8,0]
["6AV72445BA101PT0","SIMATIC IPC 477D, 15\" TOUCH, MIT WINCC FLEX SW PACKAGE",4872,"TEM",1,"Simatic",8,0]
["6AV72445DA300YA0","SIMATIC IPC477D OEM 19\" TOUCH DISPLAY, WITH CONFIGURATION: 6AV7240-.D...-.... WITH EXPRESS-DESIGN",4379,"TEM",1,"Simatic",8.8000000000000007,0]
["6AV72445EA020HB0","SIMATIC IPC477D OEM 22\" TOUCH DISPLAY, WITH CONFIGURATION: 6AV7240-6EC07-0HA0 TRUMPF DESIGN",4504,"TEM",1,"Simatic",10.14,0]
["6AV72446XX000TEM0","MOTHERBOARD COMPUTER KIT V2 CONSISTING OF: MOTHERBOARD WITH CORE I7-3517UE W/O FIELDBUS, 8 GB RAM, 160 GB SSD, WES7 P (LICENSE ONLY), INCL. BATTERY",1759,"TEM",1,"Simatic",2,0]
["6AV72446XX010TEM0","MOTHERBOARD COMPUTER KIT V1 CONSISTING OF: MOTHERBOARD WITH CORE I7-3517UE W/O FIELDBUS, 4 GB RAM, 80 GB SSD, WES7 P (LICENSE ONLY), INCL. BATTERY",1592,"TEM",1,"Simatic",2,0]
["6AV72446XX020TEM0","MOTHERBOARD COMPUTER KIT V5 CONSISTING OF: MOTHERBOARD WITH CORE I7-3517UE W/O FIELDBUS, 8 GB RAM, 160 GB SSD, WIN 7 ULTIMATE (LICENSE ONLY), INCL. BATTERY",1826,"TEM",1,"Simatic",2,0]
["6AV72446XX100TEM0","MOTHERBOARD COMPUTER KIT V4 CONSISTING OF: MOTHERBOARD WITH CORE I7-3517UE W/O FIELDBUS, 8 GB RAM, 300 GB SSD, WES7 P (LICENSE ONLY), INCL. BATTERY",1960,"TEM",1,"Simatic",2,0]
["6AV72446XX110TEM0","MOTHERBOARD COMPUTER KIT V3 CONSISTING OF: MOTHERBOARD WITH CORE I7-3517UE W/O FIELDBUS, 4 GB RAM, 80 GB SSD, WIN 7 ULTIMATE (LICENSE ONLY), INCL. BATTERY",1669,"TEM",1,"Simatic",0.65100000000000002,0]
["6AV72446XX200TEM0","MOTHERBOARD COMPUTER KIT V6 CONSISTING OF: MOTHERBOARD WITH CORE I7-3517UE W/O FIELDBUS, 8 GB RAM, 300 GB SSD, WIN 7 ULTIMATE (LICENSE ONLY), INCL. BATTERY",2027,"TEM",1,"Simatic",2,0]
["6AV72447BA000FP0","OEM OPERATOR PANEL SIMATIC IPC 477D, 15\" TOUCH 4 USB (BACK) + 1 USB (FRONT) ETHERNET (10/100/1000) PROCESSOR: CORE I7-3517UE 2 X GBIT ETHERNET (IE/PN) MEMORY EXTENSION: 8 GB EXTENSION (HW): 1X RS232; W/O PCIE; OPERATING SYSTEM: WIN7 ULTIMATE 64BIT MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE MASS STORAGE INTERNAL: SSD 160 GB STANDARD (MLC); W/O SIMATIC SOFTWARE DC24V INDUSTR. POWER SUPPLY SITOP PSU100S 24 V/10 A SITOP UPS500S",15673,"TEM",1,"Simatic",50,0]
["6AV72503EC070HA0","SIMATIC IPC 477D PRO, FULLY ENCLOSED IP65; 19\" MULTITOUCH (1366 X 768); SUITABLE FOR SUPPORT ARM W/O EXTENSION COMPONENTS (FLANGE AT TOP); 4USB (BACK); W/O USB (FRONT); ETHERNET (10/100/1000); DC24V INDUSTR. POWER SUPPLY; PROCESSOR: CORE I3-3217UE; (2C/4T, 1,6GHZ, 3MB CACHE); 2 X GBIT ETHERNET (IE/PN); MEMORY EXTENSION: 4 GB; EXTENSION (HW): 1X RS232; OPERATING SYSTEM: WINDOWS 7 ULTIMATE SP1, 64BIT; MUI (GE/EN/FR/IT); MASS STORAGE CHANGEABLE: W/O MASS STORAGE CHANGEABLE; MASS STORAGE INTERNAL: SSD 80 GB SATA; W/O SIMATIC SOFTWARE;",4326,"TEM",1,"Simatic",7.9,0]
["6AV72543DD000AS0","OPERATOR STAT. OEM IPC477D PRO VERSION D, SIMATIC IPC477D PRO, 19\" TOUCH, CELERON U827E WIN EMBEDDED STANDARD 7, REMOTE OPERATE CLIENT V 4.0, D /38/VN54X_/KB VN54X CRAFTER WRZESNIA",6470,"TEM",1,"Simatic",39,0]
["6AV72600BE210BX3","SIMATIC IPC677D, 2X10/100/1000 MBIT/S ETHERNET; 4XUSB V3.0, 1 X SERIAL (COM1); WATCHDOG, TEMPERATURE AND FAN CONTROL; RAID-CONTROLLER ON BOARD; 15\" TOUCH (1280X800); WITH FRONT USB; CELERON G1820TE (2C/2T, 2,2GHZ, 2MB CACHE); PROFIBUS/MPI (CP5622-COMPATIBLE); 2 MB BUFFERED SRAM; 500 GB HDD SATA; DVD+/-RW; 4 GB DDR3 1600 DIMM; 1 X PCIE (X16); 1 X  PCI; W/O EXTENSION (HW); WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); AC 110/230V INDUSTRIAL POWER SUPPLY WITH NAMUR; POWER CORD USA;",4403,"TEM",1,"Simatic",17,1]
["6AV72600DB200AX6","SIMATIC IPC677D, 2X10/100/1000 MBIT/S ETHERNET; 4XUSB V3.0, 1 X SERIAL (COM1); WATCHDOG, TEMPERATURE AND FAN CONTROL; RAID-CONTROLLER ON BOARD; 15\" TOUCH (1280X800); WITH FRONT USB; CORE I3-4330TE (2C/4T, 2.4GHZ, 4MB CACHE, VT-X); 250 GB HDD SATA; DVD+/-RW; 4 GB DDR3 1600 DIMM; 2 X  PCI; W/O EXTENSION (HW); WINDOWS 7 ULTIMATE 32BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); DC 24V  INDUSTRAL- POWER SUPPLY; DC 24V  INDUSTRAL- POWER SUPPLY;",4288,"TEM",1,"Simatic",17,1]
["6AV72600GA300BX3","SIMATIC IPC677D, 2X10/100/1000 MBIT/S ETHERNET; 4XUSB V3.0, 1 X SERIAL (COM1); WATCHDOG, TEMPERATURE AND FAN CONTROL; RAID-CONTROLLER ON BOARD; 15\" TOUCH (1280X800); WITH FRONT USB; XEON E3-1268LV3 (4C/8T, 2,3(3.3)GHZ, 8MB CACHE VT-D, AMT); 250 GBYTE HDD SATA; 8 GB DDR3 1600 DIMM; 2 X  PCI; W/O EXTENSION (HW); WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); AC 110/230V INDUSTRIAL POWER SUPPLY WITH NAMUR; POWER CORD USA;",4666,"TEM",1,"Simatic",17,1]
["6AV72601GA300BX3","SIMATIC IPC677D, 2X10/100/1000 MBIT/S ETHERNET; 4XUSB V3.0, 1 X SERIAL (COM1); WATCHDOG, TEMPERATURE AND FAN CONTROL; RAID-CONTROLLER ON BOARD; 19\" TOUCH (1366X768); WITH FRONT USB; XEON E3-1268LV3 (4C/8T, 2,3(3.3)GHZ, 8MB CACHE VT-D, AMT); 250 GBYTE HDD SATA; 8 GB DDR3 1600 DIMM; 2 X  PCI; W/O EXTENSION (HW); WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); AC 110/230V INDUSTRIAL POWER SUPPLY WITH NAMUR; POWER CORD USA;",4876,"TEM",1,"Simatic",17,1]
["6AV72601JM310BX0","SIMATIC IPC677D, 2X10/100/1000 MBIT/S ETHERNET; 4XUSB V3.0, 1 X SERIAL (COM1); WATCHDOG, TEMPERATURE AND FAN CONTROL; RAID-CONTROLLER ON BOARD; 19\" TOUCH (1366X768); WITH FRONT USB; XEON E3-1268LV3 (4C/8T, 2.3(3.3)GHZ, 8MB CACHE VT-D, AMT); PROFINET (IRT, 3 PORTS, CP1616-COMPATIBLE); 2 MB BUFFERED SRAM; SOLID STATE DRIVE 240 GB; 8 GB DDR3 1600 DIMM; 1 X PCIE (X16); 1 X  PCI; W/O EXTENSION (HW); WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); AC 110/230V INDUSTRIAL POWER SUPPLY WITH NAMUR; POWER CORD EUROPE;",5968,"TEM",1,"Simatic",17,1]
["6AV72602DB320AX6","SIMATIC HMI IPC677D, 2X10/100/1000 MBIT/S ETHERNET; 4XUSB V3.0, 1 X SERIAL (COM1); WATCHDOG, TEMPERATURE AND FAN CONTROL; RAID-CONTROLLER ON BOARD; 22\" TOUCH (1920 X 1080); WITH FRONT USB; CORE I3-4330TE (2C/4T, 2.4GHZ, 4MB CACHE, VT-X); 250 GB HDD SATA; DVD+/-RW; 8 GB DDR3 1600 DIMM; 1 X PCIE (X16); 1 X PCIE (X4); W/O EXTENSION (HW); WINDOWS 7 ULTIMATE 32BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); DC 24V  INDUSTRAL- POWER SUPPLY;",5138,"TEM",1,"Simatic",17,1]
["6AV72602EA300BX3","SIMATIC HMI IPC677D, 2X10/100/1000 MBIT/S ETHERNET; 4XUSB V3.0, 1 X SERIAL (COM1); WATCHDOG, TEMPERATURE AND FAN CONTROL; RAID-CONTROLLER ON BOARD; 22\" TOUCH (1920 X 1080); WITH FRONT USB; CORE I3-4330TE (2C/4T, 2.4GHZ, 4MB CACHE, VT-X); PROFIBUS/MPI CP5622-COMPATIBLE); 2 MB BUFFERED SRAM; 250 GBYTE HDD SATA; 8 GB DDR3 1600 DIMM; 2 X  PCI; W/O EXTENSION (HW); WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); AC 110/230V INDUSTRIAL POWER SUPPLY WITH NAMUR; POWER CORD USA;",5075,"TEM",1,"Simatic",17,1]
["6AV72602FD301BX6","SIMATIC HMI IPC677D, 2X10/100/1000 MBIT/S ETHERNET; 4XUSB V3.0, 1 X SERIAL (COM1); WATCHDOG, TEMPERATURE AND FAN CONTROL; RAID-CONTROLLER ON BOARD; 22\" TOUCH (1920 X 1080); WITH FRONT USB; CORE I3-4330TE (2C/4T, 2.4GHZ, 4MB CACHE, VT-X); PROFINET (IRT, 3 PORTS, CP1616-COMPATIBLE); 2 MB BUFFERED SRAM; 500 GB HDD SATA; 8 GB DDR3 1600 DIMM; 2 X  PCI; 2X USB ADDITIV 1 SLOT OCCUPIED; WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); DC 24V  INDUSTRAL- POWER SUPPLY;",5653,"TEM",1,"Simatic",17,1]
["6AV72602FH311BC3","SIMATIC HMI IPC677D, 2X10/100/1000 MBIT/S ETHERNET; 4XUSB V3.0, 1 X SERIAL (COM1); WATCHDOG, TEMPERATURE AND FAN CONTROL; RAID-CONTROLLER ON BOARD; 22\" TOUCH (1920 X 1080); WITH FRONT USB; CORE I3-4330TE (2C/4T, 2.4GHZ, 4MB CACHE, VT-X); PROFINET (IRT, 3 PORTS, CP1616-COMPATIBLE); 2 MB BUFFERED SRAM; RAID1 2 X 320 GB SATA (2,5\"); DVD+/-RW; 8 GB DDR3 1600 DIMM; 1 X PCIE (X16); 1 X  PCI; 2X USB ADDITIV 1 SLOT OCCUPIED; WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); SIMATIC IPC DIAGMONITOR V4.5 & IMAGE&PARTITION CREATOR V3.4 ADDED; AC 110/230V INDUSTRIAL POWER SUPPLY WITH NAMUR; POWER CORD USA;",6545,"TEM",1,"Simatic",17,1]
["6AV72602GD401BX6","SIMATIC HMI IPC677D, 2X10/100/1000 MBIT/S ETHERNET; 4XUSB V3.0, 1 X SERIAL (COM1); WATCHDOG, TEMPERATURE AND FAN CONTROL; RAID-CONTROLLER ON BOARD; 22\" TOUCH (1920 X 1080); WITH FRONT USB; XEON E3-1268LV3 (4C/8T, 2,3(3.3)GHZ, 8MB CACHE VT-D, AMT); 500 GB HDD SATA; 16 GB DDR3 1600 DIMM; 2 X  PCI; 2X USB ADDITIV 1 SLOT OCCUPIED; WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); DC 24V  INDUSTRAL- POWER SUPPLY;",5810,"TEM",1,"Simatic",17,1]
["6AV72602GM410BX6","SIMATIC HMI IPC677D, 2X10/100/1000 MBIT/S ETHERNET; 4XUSB V3.0, 1 X SERIAL (COM1); WATCHDOG, TEMPERATURE AND FAN CONTROL; RAID-CONTROLLER ON BOARD; 22\" TOUCH (1920 X 1080); WITH FRONT USB; XEON E3-1268LV3 (4C/8T, 2,3(3.3)GHZ, 8MB CACHE VT-D, AMT); SOLID STATE DRIVE 240 GB; 16 GB DDR3 1600 DIMM; 1 X PCIE (X16); 1 X  PCI; W/O EXTENSION (HW); WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); DC 24V  INDUSTRAL- POWER SUPPLY;",6115,"TEM",1,"Simatic",17,1]
["6AV72602GY310BX6","SIMATIC HMI IPC677D, 2X10/100/1000 MBIT/S ETHERNET; 4XUSB V3.0, 1 X SERIAL (COM1); WATCHDOG, TEMPERATURE AND FAN CONTROL; RAID-CONTROLLER ON BOARD; 22\" TOUCH (1920 X 1080); WITH FRONT USB; XEON E3-1268LV3 (4C/8T, 2,3(3.3)GHZ, 8MB CACHE VT-D, AMT); SOLID STATE DRIVE 160 GB; 8 GB DDR3 1600 DIMM; 1 X PCIE (X16); 1 X  PCI; W/O EXTENSION (HW); WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); DC 24V  INDUSTRAL- POWER SUPPLY;",5674,"TEM",1,"Simatic",17,1]
["6AV72604DM500XX3","SIMATIC HMI IPC677D, 2X10/100/1000 MBIT/S ETHERNET; 4XUSB V3.0, 1 X SERIAL (COM1); WATCHDOG, TEMPERATURE AND FAN CONTROL; RAID-CONTROLLER ON BOARD; 19\" MULTITOUCH (1366 X 768); CORE I3-4330TE (2C/4T, 2.4GHZ, 4MB CACHE, VT-X); SOLID STATE DRIVE 240 GB; 8 GB DDR3 1600 DIMM; ECC; 2 X  PCI; W/O EXTENSION (HW); W/O OPERATING SYSTEM; W/O  EXTENSION (SW); AC 110/230V INDUSTRIAL POWER SUPPLY WITH NAMUR; POWER CORD USA;",4907,"TEM",1,"Simatic",17,1]
["6AV72604HG100BX3","SIMATIC HMI IPC677D, 2X10/100/1000 MBIT/S ETHERNET; 4XUSB V3.0, 1 X SERIAL (COM1); WATCHDOG, TEMPERATURE AND FAN CONTROL; RAID-CONTROLLER ON BOARD; 19\" MULTITOUCH (1366 X 768); XEON E3-1268LV3 (4C/8T, 2.3(3.3)GHZ, 8MB CACHE VT-D, AMT); PROFIBUS/MPI CP5622-COMPATIBLE); 2 MB BUFFERED SRAM; RAID1 2 X 320 GB SATA (2,5\"); 2 GB DDR3 1600 DIMM; 2 X  PCI; W/O EXTENSION (HW); WINDOWS 7 ULTIMATE 64BIT SP1, MUI (EN, GE, FR, IT, SP); W/O  EXTENSION (SW); AC 110/230V INDUSTRIAL POWER SUPPLY WITH NAMUR; POWER CORD USA;",5579,"TEM",1,"Simatic",17,1]
["6AV72643AA000BK0","DAIMLER IW5, PLC CONTROL CABINET, STAGE OF EXPANSION 1, CONTAINS: CABINET 600MM RAL7035, 1X SIMATIC S7-319F, 1X SCALANCE XM416-4C, 1X PN/PN COUPLER, 1X FIREWALL, SITOP PSU8200 24 V/20 A",15841,"TEM",1,"Simatic",140,0]
["6AV72643AA010BK0","DAIMLER IW5, PLC CONTROL CABINET, CONVEYANCE/ FITTING, STAGE OF EXPANSION 1, CONTAINS: CABINET 600MM RAL7035, 1X SIMATIC S7-319F, 1X SCALANCE XM416-4C, 1X SCALANCE X208, 1X PN/PN COUPLER, 1X FIREWALL, SITOP PSU8200 24 V/20 A",16587,"TEM",1,"Simatic",140,0]
["6AV72643AB000BK0","DAIMLER IW5, PLC CONTROL CABINET, STAGE OF EXPANSION 2, CONTAINS: CABINET 600MM RAL7035, 2X SIMATIC S7-319F, 2X SCALANCE XM416-4C, 2X PN/PN COUPLER, 2X FIREWALL, SITOP PSU8200 24 V/20 A",27087,"TEM",1,"Simatic",140,0]
["6AV72643AC000BK0","DAIMLER IW5, PLC CONTROL CABINET, STAGE OF EXPANSION 3, CONTAINS: CABINET 600MM RAL7035, 3X SIMATIC S7-319F, 3X SCALANCE XM416-4C, 3X PN/PN COUPLER, 3X FIREWALL, SITOP PSU8200 24 V/20 A",38365,"TEM",1,"Simatic",156,0]
["6AV72643BM030AA0","Bundle SIMATIC Flat Panel 19T 19\" touch TFT display, 1280 X 1024 pixel resolution, 24V DC and 120/240V AC, VGA, DVI-D interface, incl. VGA cable 1.8m, incl. induSTrial DVI-D 3m cable incl. induSTrial USB 3m cable,",2194,"TEM",1,"Simatic",5.0999999999999996,0]
["6AV72643DA020AS0","OPERATOR STAT. OEM IPC677D VERS A W. BASIC PACK S7-319F SIMATIC IPC677D, 19\" TOUCH, XEON E3-1268LV3, (4C/8T, 2,3(3,3)GHZ, W/O OPERATING SYSTEM STEP7 + WINCC FLEXIBLE, A /38/VN54X_/KB, CPU319F VN54X CRAFTER WRZESNIA",17690,"TEM",1,"Simatic",60,0]
["6AV74115AC001VS0","VIESSMANN PACKAGE 1 9 INCH CONSISTING OF: SIMATIC IPC 277E, 9\" TOUCH, BLACK FRONT (6AV7411-5AC00-0VS0); COL WINCC RT ADVANCED 2048PT, V13; COL WINCC RECEIPES + LOGGING",3444,"TEM",1,"Simatic",4.2,0]
["6AV74124AD000YA0","SIMATIC IPC277D OEM 9\" TOUCH TFT DISPLAY, WITH CONFIGURATION: 6AV7881-2A.00-...0 WITH EXPRESS-DESIGN",2098,"TEM",1,"Simatic",2.5,0]
["6AV74125AA001FW0","SIMATIC IPC277E, 12\" TOUCH BUNDLE, CUSTOMER-SPECIFIC DESIGN B AND  WINCC FLEXIBLE RT 512, OPTION ARCHIVES, CPU ET 200S PN 151-8, MMC 512 KBYTE, TERMINAL MODULE, POWER MODULE, FOR CUSTOMER FLOTTWEG SE ONLY",5688,"TEM",1,"Simatic",4,0]
["6AV74134AB000FW1","SIMATIC IPC277D, 12\" TOUCH BUNDLE, CUSTOMER-SPECIFIC DESIGN B AND  WINCC FLEXIBLE RT 512, OPTION ARCHIVES, CPU ET 200S PN 151-8, MMC 512 KBYTE, TERMINAL MODULE, POWER MODULE, FOR CUSTOMER FLOTTWEG SE ONLY",2474,"TEM",1,"Simatic",4,0]
["6AV74134AD000YD0","SIMATIC IPC277D OEM 12\" TOUCH TFT DISPLAY, WITH EXPRESS-DESIGN WITH CONFIGURATION: BASIS: 6AV7881-3AF00-3DB0 ATOM E660 (1,3 GHZ), 2GB RAM; 8 GB SIMATIC PC COMPACTFLASH; WES 7 SP1 (CF >= 4 GB/SSD); WINAC RTX 2010; CUSTOMER DESIGN -> INNOMATEC",3211,"TEM",1,"Simatic",3.3,0]
["6AV74134AD000YE0","SIMATIC IPC277D OEM 12\" TOUCH TFT DISPLAY, WITH EXPRESS-DESIGN WITH CONFIGURATION: BASIS: 6AV7881-3AF00-3DA0; ATOM E660 (1.3 GHZ), 2GB RAM; 8 GB SIMATIC PC COMPACTFLASH; WES 7 SP1 (CF => 4 GB/SSD); W/O SIMATIC SOFTWARE; CUSTOMER -DESIGN -> INNOMATEC",2613,"TEM",1,"Simatic",3.3,0]
["6AV74222CB030AS0","VW416 CHATTANOOGA C/62/VW416 CHATTANOOGA/KB OPERATOR STAT. OEM MP 377 PRO VAR C REMOTE OPERATE 15\" TOUCH WITH HOUSING ANCHORAGE, WITH SW REMOTE OPERATE V3.1, CLIENT INSTALLED,",3458,"TEM",1,"Simatic",10,0]
["6AV74243BB020AS0","OPERATOR STAT. OEM IPC677D VERS A W. BASIC PACK S7-319F SIMATIC IPC677D, 19\" TOUCH, XEON E3-1268LV3, (4C/8T, 2.3(3.3)GHZ), WIN 7 ULTIMATE 64BIT, MUI + STEP7 + WINCC FLEXIBLE, VW A/37/PO536_BRATISLAVA PO536 BRATISLAVA",15219,"TEM",1,"Simatic",60,0]
["6AV74243BB050AS0","OPERATOR STAT. OEM IPC677D VERSION F, SIMATIC IPC677D, 19\" TOUCH, XEON E3-1268LV3, (4C/8T, 2.3(3.3)GHZ), WIN 7 ULTIMATE 64BIT,  MUI, VW F/37/PO536_BRATISLAVA PO536 BRATISLAVA",7070,"TEM",1,"Simatic",60,0]
["6AV74243ND020AS0","OPERATOR STATION OEM IPC677D, AU58X NECKARSULM A /22/AU58X/KB NECKARSULM, VERSION A W/O CPU, SIMATIC IPC677D, 19\"  TOUCH, XEON E3-1268LV3, (4C/8T, 2.3(3.3)GHZ), WIN 7 ULTIMATE 64BIT,  MUI + STEP7 + WINCC, NOTE! ORDERABLE ONLY WITH BY-PACK KIT 6AV7424-3ND02-0AS1",8790,"TEM",1,"Simatic",60,0]
["6AV74243ND020AS1","BY-PACK KIT VERSION A, AU58X NECKARSULM 22/AU58X/KB NECKARSULM, VERSION A WITH CPU 319F AND SCALANCE, SIPLUG",8452,"TEM",1,"Simatic",4,0]
["6AV74243ND050AS0","OPERATOR STATION OEM IPC677D, AU58X NECKARSULM F /22/AU58X/KB NECKARSULM, VERSION F, SIMATIC IPC677D, 19\"  TOUCH, XEON E3-1268LV3, (4C/8T, 2.3(3.3)GHZ), WIN 7 ULTIMATE 64BIT,  MUI",7019,"TEM",1,"Simatic",60,0]
["6AV74243PA020AS0","OPERATOR STAT. OEM IPC677D VERS A W. BASIC PACK S7-319F SIMATIC IPC677D, 19\" TOUCH, XEON E3-1268LV3, (4C/8T, 2.3(3.3)GHZ),  WIN 7 ULTIMATE 64BIT, MUI + STEP7 + WINCC FLEXIBLE, SOFTWARE IMAGE VW INSTALLED VW270/SE27X_PAMPLONA_MARTORELL VW PAMPLONA",15167,"TEM",1,"Simatic",60,0]
["6AV74243PA050AS0","OPERATOR STAT. OEM IPC677D VERSION F, SIMATIC IPC677D, 19\" TOUCH, XEON E3-1268LV3, (4C/8T, 2.3(3.3)GHZ), WIN 7 ULTIMATE 64BIT,  MUI, SOFTWARE IMAGE VW INSTALLED VW270/SE27X_PAMPLONA_MARTORELL VW PAMPLONA",7019,"TEM",1,"Simatic",60,0]
["6AV74243PA060AS0","OPERATOR STAT. OEM IPC677D VERS I W. BASIC PACK S7-319F SIMATIC IPC677D, 19\" TOUCH, XEON E3-1268LV3, (4C/8T, 2.3(3.3)GHZ),  WIN 7 ULTIMATE 64BIT, MUI + STEP7 + WINCC V7.3, RT65536, SOFTWARE IMAGE VW INSTALLED VW270/SE27X_PAMPLONA_MARTORELL VW PAMPLONA",17674,"TEM",1,"Simatic",60,0]
["6AV74243SB020AS0","OPERATOR STAT. OEM IPC677D VERS A W. BASIC PACK S7-319F SIMATIC IPC677D, 19\" TOUCH, XEON E3-1268LV3, (4C/8T, 2.3(3.3)GHZ),  WIN 7 ULTIMATE 64BIT, MUI + STEP7 + WINCC FLEXIBLE, SOFTWARE IMAGE VW INSTALLED VW SVW FAW CHINA",15167,"TEM",1,"Simatic",63,0]
["6AV74243SB050AS0","OPERATOR STAT. OEM IPC677D VERSION F, SIMATIC IPC677D, 19\" TOUCH, XEON E3-1268LV3, (4C/8T, 2.3(3.3)GHZ), WIN 7 ULTIMATE 64BIT,  MUI, SOFTWARE IMAGE VW INSTALLED VW SVW FAW CHINA",7019,"TEM",1,"Simatic",63,0]
["6AV74243UA020AS0","OPERATOR STAT. OEM IPC677D VERS A W. BASIC PACK S7-319F SIMATIC IPC677D, 19\" TOUCH, XEON E3-1268LV3, (4C/8T, 2.3(3.3)GHZ),  WIN 7 ULTIMATE 64BIT, MUI + STEP7 + WINCC FLEXIBLE, SOFTWARE IMAGE VW INSTALLED VW270 UITENHAGE",15167,"TEM",1,"Simatic",60,0]
["6AV74243UA050AS0","OPERATOR STAT. OEM IPC677D VERSION F, SIMATIC IPC677D, 19\" TOUCH, XEON E3-1268LV3, (4C/8T, 2.3(3.3)GHZ), WIN 7 ULTIMATE 64BIT,  MUI, SOFTWARE IMAGE VW INSTALLED VW270 UITENHAGE",7019,"TEM",1,"Simatic",60,0]
["6AV74284AD120BK0","DAIMLER IW5, INTEGRA IPC227E NANOBOX, CELERON N2807 (2C/2T), 2 GB RAM, 80 GB SSD, 2 X GIGABIT ETHERNET, 1 X USB3.0, 3X USB2.0, WIN7 ULTIMATE 32 BIT SP1, MIT IMAGE INTEGRA HVO52",1876,"TEM",1,"Simatic",6,1]
["6AV74284AD130BK0","DAIMLER IW5, INTEGRA IPC227E NANOBOX, CELERON N2807 (2C/2T), 2 GB RAM, 80 GB SSD, 2 X GIGABIT ETHERNET, 1 X USB3.0, 3X USB2.0, WIN7 ULTIMATE 32 BIT SP1, MIT IMAGE INTEGRA STANDALONE",1876,"TEM",1,"Simatic",6,1]
["6AV74286AD300BK0","DAIMLER IW5, INTEGRA IPC627D BOX, XEON E3-1268LV3, 4 GB DDR3 1066 DIMM, 250 GBYTE HDD SATA, W/O OPTICAL DRIVE, 2 X GIGABIT ETHERNET, 4 X USB V3.0, 1 X SERIAL (COM1), WITH PROFIBUS/MPI, 2 X PCI, 2X USB ADDITIONAL, WIN7 ULTIMATE 32 BIT SP1, WITH IMAGE INTEGRA PN",6174,"TEM",1,"Simatic",6,1]
["6AV74286AD310BK0","DAIMLER IW5, INTEGRA IPC627D BOX, XEON E3-1268LV3, 4 GB DDR3 1066 DIMM, 250 GBYTE HDD SATA, W/O OPTICAL DRIVE, 2 X GIGABIT ETHERNET, 4 X USB V3.0, 1 X SERIAL (COM1), WITH PROFIBUS/MPI, 2 X PCI, 2X USB ADDITIONAL, WIN7 ULTIMATE 32 BIT SP1, WITH IMAGE INTEGRA TECH",3964,"TEM",1,"Simatic",6,1]
["6AV74300AL000FA3","FIAT SCP 1 WIN7 SYSTEM CONTROL PANEL 1 WITH FP 19\"PRO, EXT.UNIT SIMATIC IPC627C, WIN7 (64), 8GB LIC. WIN CC RT 8192 TAG LIC SIMATIC NET SOFTNET S7 V8.1 CPU319F-3, CP343-1 ADV SCALANCE X216, ET200S",28277,"TEM",1,"Simatic",178,0]
["6AV74300AL000FA4","FIAT SCP 1 WIN7 V2, SYSTEM CONTROL PANEL 1, WITH FP 19\"PRO, EXT.UNIT + KP8F SIMATIC IPC627C, WIN7 (64), 8GB LIC. WIN CC RT 8192 TAG, LIC SIMATIC NET SOFTNET S7 V8.2 CPU319F-3, CP343-1 ADV, SCALANCE 2X X208",28276,"TEM",1,"Simatic",180,0]
["6AV74300AL000FA5","FIAT SCP 1 WIN7 V2.1, SYSTEM CONTROL PANEL 1, WITH FP 19\"PRO, EXT.UNIT + KP8F SIMATIC IPC627C, WIN7 (64), 8GB LIC. WIN CC V7.3 RT 8192 TAG, LIC SIMATIC NET SOFTNET S7 V12 CPU319F-3, CP343-1 ADV, SCALANCE 2X X208 SITOP PSU8200 + PSE201U BUFFER MODULE",28518,"TEM",1,"Simatic",177,0]
["6AV74300AL002FA2","FIAT SCP 2 SYSTEM CONTROL PANEL 2 CPU319F-3, CP343-1 ADV SCALANCE X216, ET200S",12673,"TEM",1,"Simatic",177,0]
["6AV74300AL002FA4","FIAT SCP 2 V2, SYSTEM CONTROL PANEL 2, CPU319F-3, CP343-1 ADV, SCALANCE 2X X208",12501,"TEM",1,"Simatic",150,0]
["6AV74300AL002FA5","FIAT SCP 2 V2.1, SYSTEM CONTROL PANEL 2, CPU319F-3, CP343-1 ADV, SCALANCE 2X X208 SITOP PSU8200 + PSE201U BUFFER MODULE",12742,"TEM",1,"Simatic",154,0]
["6AV74300AL223FA3","FIAT SCP 3 WIN7 SYSTEM CONTROL PANEL 3 WITH FP 19\"PRO, EXT.UNIT SIMATIC IPC627C, WIN7 (64), 8GB LIC. WIN CC RT 8192 TAG LIC SIMATIC NET SOFTNET S7 V8.1 2X CPU319F-3, 2X CP343-1 ADV 2X SCALANCE X216, ET200S",36207,"TEM",1,"Simatic",182,0]
["6AV74300AL223FA4","FIAT SCP 3 WIN7 V2, SYSTEM CONTROL PANEL 3, WITH FP 19\"PRO, EXT.UNIT + KP8F SIMATIC IPC627C, WIN7 (64), 8GB LIC. WIN CC RT 8192 TAG, LIC SIMATIC NET SOFTNET S7 V8.2 2X CPU319F-3, 2X CP343-1 ADV, 4X SCALANCE X208",36207,"TEM",1,"Simatic",162,0]
["6AV74300AL223FA5","FIAT SCP 3 WIN7 V2.1, SYSTEM CONTROL PANEL 3, WITH FP 19\"PRO, EXT.UNIT + KP8F SIMATIC IPC627C, WIN7 (64), 8GB LIC. WIN CC V7.3 RT 8192 TAG, LIC SIMATIC NET SOFTNET S7 V12 2X CPU319F-3, 2X CP343-1 ADV, 4X SCALANCE X208 SITOP PSU8200 + PSE201U BUFFER MODULE",36448,"TEM",1,"Simatic",180,0]
["6AV74300AL224FA2","FIAT SCP 4 SYSTEM CONTROL PANEL 4 2X CPU319F-3, 2X CP343-1 ADV 2X SCALANCE X216, ET200S",20604,"TEM",1,"Simatic",177,0]
["6AV74300AL224FA4","FIAT SCP 4 V2, SYSTEM CONTROL PANEL 4, 2X CPU319F-3, 2X CP343-1 ADV, 4X SCALANCE X208",20344,"TEM",1,"Simatic",160,0]
["6AV74300AL224FA5","FIAT SCP 4 V2.1, SYSTEM CONTROL PANEL 4, 2X CPU319F-3, 2X CP343-1 ADV, 4X SCALANCE X208, SITOP PSU8200 + PSE201U BUFFER MODULE",20587,"TEM",1,"Simatic",60,0]
["6AV74645AA043AT3","IPC477D PRO BUNDLE FULLY ENCLOSED IP65; 19\" MULTITOUCH (1366 X 768); SUPPORT ARM VARIANT; 4USB (BACK); W/O USB (FRONT); 2 X GBIT ETHERNET (IE/PN); DC24V INDUSTR. POWER SUPPLY; CORE I3-3217UE; (2C/4T, 1.6GHZ) 4 GB RAM, 1 X RS232, WIN 7 ULTIMATE SP1, 64BIT MUI PREINSTALLED ON SSD 80GB W/O SIMATIC SOFTWARE WITH BASE ADAPTER",5018,"TEM",1,"Simatic",8.5,0]
["6AV74653BA201BK0","DAIMLER IW5, HVO 57, PROFINET, CASE WITH SIMATIC IPC277E/ 9\" TOUCH IMAGE INTEGRA HVO57",3426,"TEM",1,"Simatic",10.5,0]
["6AV74735CA060BK0","DAIMLER IW5, OPERATOR STATION INTEGRA EBF PN STAGE OF EXPANSION50, GERMAN, SIMATIC IFP1900 MT, SIMATIC IPC627D, XEON E3-1268LV3, PROFIBUS/MPI, 250 GBYTE HDD SATA, 4 GB DDR3 1600 DIMM, WINDOWS 7 ULTIMATE 32BIT SP1, DC 24V, SCALANCE XF204, KEYBOARD GER, SIMATIC HMI KP32F PN, EUCHNER KEY EKS, INTEGRA DESIGNER PRO IMAGE INTEGRA PN",17697,"TEM",1,"Simatic",80,0]
["6AV74735CA260BK0","DAIMLER IW5, COMP. CONT. CABINET GERMAN SIMATIC IFP1900 MT SIMATIC IPC627D XEON E3-1268LV3 PROFIBUS/MPI 250 GBYTE HDD SATA 4 GB DDR3 1600 DIMM WINDOWS 7 ULTIMATE SIMATIC HMI KP32F PN KEYBOARD GER EUCHNER KEY EKS SCALANCE XM416-4C PN/PN KOPPLER FIREWALL DIF.SWITCHGEAR ET200S CONFIGURATION CLIMATE CONTROL UNIT IMAGE INTEGRA PN",38523,"TEM",1,"Simatic",220,0]
["6AV74735CA500BK0","DAIMLER IW5, OPERATOR STATION EBF FOR QS SYSTEMS GERMAN SIMATIC IFP2200 MT SIMATIC IPC627D XEON E3-1268LV3 PROFIBUS/MPI CP5622-COMPATIBLE); 250 GBYTE HDD SATA 4 GB DDR3 1600 DIMM WINDOWS 7 ULTIMATE 32BIT SP1 DC 24V SCALANCE XF204 KEYBOARD GER EUCHNER KEY EKS IMAGE INTEGRA TECH",14291,"TEM",1,"Simatic",105,0]
["6AV74735CA530BK0","DAIMLER IW5, OPERATOR STATION INTEGRA EBF PN STAGE OF EXPANSION53 GERMAN SIMATIC IFP1900 MT SIMATIC IPC627D XEON E3-1268LV3 PROFIBUS/MPI 250 GBYTE HDD SATA 4 GB DDR3 1600 DIMM WINDOWS 7 ULTIMATE 32BIT SP1 DC 24V SCALANCE XF204 KEYBOARD GER EUCHNER KEY EKS INTEGRA DESIGNER PRO IMAGE INTEGRA PN",15481,"TEM",1,"Simatic",80,0]
["6AV74735CA540BK0","DAIMLER IW5, OPERATOR STATION INTEGRA EBF PN STAGE OF EXPANSION53, GERMAN, SIMATIC IFP1900 MT, SIMATIC IPC627D, XEON E3-1268LV3, PROFIBUS/MPI, 250 GBYTE HDD SATA, 4 GB DDR3 1600 DIMM, WINDOWS 7 ULTIMATE, 32BIT SP1, DC 24V, SCALANCE XF204, KEYBOARD GERMAN, EUCHNER KEY EKS, IMAGE INTEGRA TECH,",13003,"TEM",1,"Simatic",80,0]
["6AV74735CA570BK0","DAIMLER IW5, OPERATOR STATION INTEGRA EBF IT SPECIAL CONFIGUARTION IT GERMAN W/O IPC W/O SOFTWARE W/O LICENCES",6323,"TEM",1,"Simatic",80,0]
["6AV74735CB060BK0","DAIMLER IW5, OPERATOR STATION INTEGRA EBF PN STAGE OF EXPANSION50, ENGLISH, SIMATIC IFP1900 MT, SIMATIC IPC627D, XEON E3-1268LV3, PROFIBUS/MPI, 250 GBYTE HDD SATA, 4 GB DDR3 1600 DIMM, WINDOWS 7 ULTIMATE, 32BIT SP1, DC 24V, SCALANCE XF204, KEYBOARD ENGLISH, SIMATIC HMI KP32F PN, EUCHNER KEY EKS, INTEGRA DESIGNER PRO, IMAGE INTEGRA PN",17697,"TEM",1,"Simatic",80,0]
["6AV74735CB260BK0","DAIMLER IW5, COMP. CONT. CABINET ENGLISH SIMATIC IFP1900 MT SIMATIC IPC627D XEON E3-1268LV3 PROFIBUS/MPI 250 GBYTE HDD SATA 4 GB DDR3 1600 DIMM WINDOWS 7 ULTIMATE SIMATIC HMI KP32F PN KEYBOARD ENG EUCHNER KEY EKS SCALANCE XM416-4C PN/PN KOPPLER FIREWALL DIF.SWITCHGEAR ET200S CONFIGURATION CLIMATE CONTROL UNIT IMAGE INTEGRA PN",38523,"TEM",1,"Simatic",120,0]
["6AV74735CB500BK0","DAIMLER IW5, OPERATOR STATION EBF FOR QS SYSTEMS ENGLISH SIMATIC IFP2200 MT SIMATIC IPC627D XEON E3-1268LV3 PROFIBUS/MPI CP5622-COMPATIBLE); 250 GBYTE HDD SATA 4 GB DDR3 1600 DIMM WINDOWS 7 ULTIMATE 32BIT SP1 DC 24V SCALANCE XF204 KEYBOARD ENG EUCHNER KEY EKS IMAGE INTEGRA TECH",14291,"TEM",1,"Simatic",105,0]
["6AV74735CB530BK0","DAIMLER IW5, OPERATOR STATION INTEGRA EBF PN STAGE OF EXPANSION53 ENGLISH SIMATIC IFP1900 MT SIMATIC IPC627D XEON E3-1268LV3 PROFIBUS/MPI 250 GBYTE HDD SATA 4 GB DDR3 1600 DIMM WINDOWS 7 ULTIMATE 32BIT SP1 DC 24V SCALANCE XF204 KEYBOARD ENG EUCHNER KEY EKS INTEGRA DESIGNER PRO IMAGE INTEGRA PN",15481,"TEM",1,"Simatic",80,0]
["6AV74735CB540BK0","DAIMLER IW5, OPERATOR STATION INTEGRA EBF PN STAGE OF EXPANSION53, ENGLISH, SIMATIC IFP1900 MT, SIMATIC IPC627D, XEON E3-1268LV3, PROFIBUS/MPI, 250 GBYTE HDD SATA, 4 GB DDR3 1600 DIMM, WINDOWS 7 ULTIMATE, 32BIT SP1, DC 24V, SCALANCE XF204, KEYBOARD ENGISH, EUCHNER KEY EKS, IMAGE INTEGRA TECH,",13003,"TEM",1,"Simatic",80,0]
["6AV74735CB570BK0","DAIMLER IW5, OPERATOR STATION INTEGRA EBF IT SPECIAL CONFIGUARTION IT ENGLISH W/O IPC W/O SOFTWARE W/O LICENCES",6323,"TEM",1,"Simatic",80,0]
["6AV74735CD060BK0","DAIMLER IW5, OPERATOR STATION INTEGRA EBF PN STAGE OF EXPANSION50,HUNGARIAN, SIMATIC IFP1900 MT, SIMATIC IPC627D, XEON E3-1268LV3, PROFIBUS/MPI, 250 GBYTE HDD SATA, 4 GB DDR3 1600 DIMM, WINDOWS 7 ULTIMATE, 32BIT SP1, 24V DC, SCALANCE XF204, KEYBOARD HUNGARIAN SIMATIC HMI KP32F PN, EUCHNER KEY EKS INTEGRA DESIGNER PRO IMAGE INTEGRA PN",17697,"TEM",1,"Simatic",80,0]
["6AV74735CD260BK0","DAIMLER IW5, COMP. CONT. CABINET HUNGARY SIMATIC IFP1900 MT SIMATIC IPC627D XEON E3-1268LV3 PROFIBUS/MPI 250 GBYTE HDD SATA 4 GB DDR3 1600 DIMM WINDOWS 7 ULTIMATE SIMATIC HMI KP32F PN KEYBOARD HUN EUCHNER KEY EKS SCALANCE XM416-4C PN/PN KOPPLER FIREWALL DIF.SWITCHGEAR ET200S CONFIGURATION CLIMATE CONTROL UNIT IMAGE INTEGRA PN",38523,"TEM",1,"Simatic",120,0]
["6AV74735CD500BK0","DAIMLER IW5, OPERATOR STATION EBF FOR QS SYSTEMS HUNGARY SIMATIC IFP2200 MT SIMATIC IPC627D XEON E3-1268LV3 PROFIBUS/MPI CP5622-COMPATIBLE); 250 GBYTE HDD SATA 4 GB DDR3 1600 DIMM WINDOWS 7 ULTIMATE 32BIT SP1 DC 24V SCALANCE XF204 KEYBOARD HUN EUCHNER KEY EKS IMAGE INTEGRA TECH",14291,"TEM",1,"Simatic",105,0]
["6AV74735CD530BK0","DAIMLER IW5, OPERATOR STATION INTEGRA EBF PN STAGE OF EXPANSION53 HUNGARY SIMATIC IFP1900 MT SIMATIC IPC627D XEON E3-1268LV3 PROFIBUS/MPI 250 GBYTE HDD SATA 4 GB DDR3 1600 DIMM WINDOWS 7 ULTIMATE 32BIT SP1 DC 24V SCALANCE XF204 KEYBOARD HUN EUCHNER KEY EKS INTEGRA DESIGNER PRO IMAGE INTEGRA PN",15481,"TEM",1,"Simatic",80,0]
["6AV74735CD540BK0","DAIMLER IW5, OPERATOR STATION INTEGRA EBF PN STAGE OF EXPANSION53,HUNGARIAN, SIMATIC IFP1900 MT, SIMATIC IPC627D, XEON E3-1268LV3, PROFIBUS/MPI, 250 GBYTE HDD SATA, 4 GB DDR3 1600 DIMM, WINDOWS 7 ULTIMATE, 32BIT SP1, DC 24V, SCALANCE XF204, KEYBOARD HUNGARIAN, EUCHNER KEY EKS, IMAGE INTEGRA TECH,",13003,"TEM",1,"Simatic",80,0]
["6AV76741KA000AA0","BASIC ADAPTER FOR ALL FULLY ENCLOSED HMI UNITS INCL. 4 SCREWS FOR MOUNTING COLOR: SILVER",95.600000000000009,"TEM",1,"Simatic",0.46,0]
["6AV78600CH300AA0","SIMATIC FLAT PANEL CABLE INDUSTRIAL GRADE USB 3M",15.8,"TEM",1,"Simatic",9.7000000000000003E-2,1]
["6AV78633AB100AA0","SIMATIC IFP1900 FLAT PANEL 19\" DISPLAY (16:9), W/O TOUCH, DISPLAY ONLY EXTENDED VERSION, MAX 30M, 1366X768 PIXEL, FOR 24V DC AND 100-240V AC, DISPLAYPORT / DVI INTERFACE INCL. DVI/USB-CABLE 1,8M",1260,"TEM",1,"Simatic",8.2200000000000006,1]
["6AV78812AA001BA0","SIMATIC IPC277D (NANOPANEL PC) 9\" TOUCH TFT; 2 X 10/100/1000 MBIT/S ETHERNET RJ45; 3 X USB V2.0 (HIGH CURRENT); 1 X SERIAL (COM1); COMPACTFLASH SLOT; 24V DC POWER SUPPLY; ATOM E640 (1,0 GHZ), 1GB RAM; STANDARD FRONT; 2 GB SIMATIC PC COMPACTFLASH; WES 2009 SP3 (CF FROM 2 GB/SSD); W/O SIMATIC SOFTWARE;",1731,"TEM",1,"Simatic",2.6,1]
["6AV78815AA008BH0","SIMATIC IPC277D (NANOPANEL PC) 19\" TOUCH TFT, FRONT USB; 2 X 10/100/1000 MBIT/S ETHERNET RJ45; 3 X USB V2.0 (HIGH CURRENT); 1 X SERIAL (COM1); COMPACTFLASH SLOT; 24V DC POWER SUPPLY; ATOM E640 (1,0 GHZ), 1GB RAM; STANDARD FRONT; 80 GB SOLID-STATE DRIVE SATA; WES 2009 SP3 (CF FROM 2 GB/SSD); WINCC ADVANCED RT V13 2048 PT (INCL. LOGGING AND RECIPES);",3952,"TEM",1,"Simatic",6.35,1]
["6ES76476CB060AX0","SIMATIC IPC627C (BOX PC), HD GRAFIK ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45; 4 X USB V2.0 (HIGH CURRENT); 1 X SERIAL (COM1); RAID-CONTROLLER ON BOARD; COMPACT FLASH DRIVE NR.1 FRONT FRONT SIDE; WATCHDOG, STP.-/FAN- MONITORING; CELERON P4505  (2C/2T, 1.86 GHZ, VT, 2MB CACHE); PROFIBUS/MPI (CP5611-A2 COMPATIBLE); 2 MB BUFFERED SRAM; 1 GB DDR3 1066 DIMM; DC 24V  INDUSTRAL- POWER SUPPLY; 2 X  PCI FREE; 250 GBYTE HDD SATA; WITHOUT OPERATION SYSTEM; WITHOUT EXTENSION (SW);",2376,"TEM",1,"Simatic",6.45,1]
["6ES76476CD660XX0","SIMATIC IPC627C (BOX PC), HD GRAFIK ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45; 4 X USB V2.0 (HIGH CURRENT); 1 X SERIAL (COM1); RAID-CONTROLLER ON BOARD; COMPACT FLASH DRIVE NR.1 FRONT FRONT SIDE; WATCHDOG, STP.-/FAN- MONITORING; CORE I3-330E (2C/4T, 2.13GHZ, HT, VT, 3MB CACHE); 4 GB DDR3 1066 DIMM; ECC; DC 24V  INDUSTRAL- POWER SUPPLY; 2 X  PCI FREE; WITHOUT DRIVES; WITHOUT OPERATION SYSTEM; WITHOUT EXTENSION (SW);",2817,"TEM",1,"Simatic",6.1,1]
["6ES76476CG130BB0","SIMATIC IPC627C (BOX PC), HD GRAFIK ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45; 4 X USB V2.0 (HIGH CURRENT); 1 X SERIAL (COM1); RAID-CONTROLLER ON BOARD; COMPACT FLASH DRIVE NR.1 FRONT FRONT SIDE; WATCHDOG, STP.-/FAN- MONITORING; CORE I7-610E (2C/4T, 2.53GHZ, TB, HT, VT, AMT, 4MB CACHE); 2 GB DDR3 1066 DIMM; AC 110/230V INDUSTRIAL POWER SUPPLY WITH NAMUR; POWER CABLE USA; 2 X  PCI FREE; 250 GBYTE HDD SATA; DVD+/-RW; WINDOWS 7 ULTIMATE 32BIT SP1, MUI (EN, GER, FR, IT, SP); WITHOUT EXTENSION (SW);",3415,"TEM",1,"Simatic",7.05,1]
["6ES76476CH300GB0","SIMATIC IPC627C (BOX PC), HD GRAFIK ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45; 4 X USB V2.0 (HIGH CURRENT); 1 X SERIAL (COM1); RAID-CONTROLLER ON BOARD; COMPACT FLASH DRIVE NR.1 FRONT FRONT SIDE; WATCHDOG, STP.-/FAN- MONITORING; CORE I7-610E (2C/4T, 2.53GHZ, TB, HT, VT, AMT, 4MB CACHE); PROFIBUS/MPI (CP5611-A2 COMPATIBLE); 2 MB BUFFERED SRAM; 4 GB DDR3 1066 DIMM; AC 110/230V INDUSTRIAL POWER SUPPLY WITH NAMUR; POWER CABLE EUROPA; 2 X  PCI FREE; RAID1 2 X 320 GB SATA (2,5\"); WINDOWS 7 ULTIMATE 32BIT SP1, MUI (EN, GER, FR, IT, SP); WITHOUT EXTENSION (SW);",4203,"TEM",1,"Simatic",6.95,1]
["6ES76476PG260BA0","SIMATIC IPC827C (BOX PC), HD GRAFIK ONBOARD, 2X10/100/1000 MBIT/S ETHERNET RJ45; 4 X USB V2.0 (HIGH CURRENT); 1 X SERIAL (COM1); RAID-CONTROLLER ON BOARD; COMPACT FLASH DRIVE NO.1 FRONT SIDE; WATCHDOG, STP.-/FAN- MONITORING; CORE I7-610E (2C/4T, 2.53GHZ, TB, HT, VT, AMT, 4MB CACHE); 3 GB DDR3 1066 DIMM; DC 24V  INDUSTRAL- POWER SUPPLY; 3 X  PCI, 1 X PCIE (X4), 1 X PCIE (X16) FREE; 250 GBYTE HDD SATA; DVD+/-RW; WINDOWS XP PROF.  SP3 MUI (EN, GER, FR, IT, SP); WITHOUT EXTENSION (SW);",3784,"TEM",1,"Simatic",7.45,1]
["6ES76478AA000AA1","SIMATIC IPC227D  (NANOBOX PC) 1 X DVI-D GRAPHIC INTERFACE; 2 X 10/100/1000 MBIT/S ETHERNET RJ45; 4 X USB V2.0 (HIGH CURRENT); COMPACTFLASH SLOT; 24V DC INDUSTRIAL POWER SUPPLY; ATOM E620 (600 MHZ), 512MB RAM; W/O DRIVE, WITH CF-SLOT; COM1: RS232; W/O OPERATING SYSTEM; W/O SIMATIC SOFTWARE; DEVICE TYPE BASE; MOUNTING ON DIN RAIL;",860,"TEM",1,"Simatic",2.4500000000000002,1]
["6ES76478AG400AB1","SIMATIC IPC227D  (NANOBOX PC) 1 X DVI-D GRAPHIC INTERFACE; 2 X 10/100/1000 MBIT/S ETHERNET RJ45; 4 X USB V2.0 (HIGH CURRENT); COMPACTFLASH SLOT; 24V DC INDUSTRIAL POWER SUPPLY; ATOM E660 (1,3 GHZ), 2GB RAM; 80 GB SOLID-STATE DRIVE SATA; COM1: RS232; W/O OPERATING SYSTEM; W/O SIMATIC SOFTWARE; DEVICE TYPE: PCIE (1 STECKPLATZ); MOUNTING ON DIN RAIL;",1459,"TEM",1,"Simatic",2.4500000000000002,1]
["6ES76482AJ400LA0","SIMATIC IPC MEMORY EXTENSION: MEMORY MODULE 1 GB (1X 1 GB), DDR3 1333 SDRAM, DIMM, FOR SIMATIC RACK IPC547D",158,"TEM",1,"Simatic",6.8000000000000005E-2,1]
["6ES76486WA010YA0","SIMATIC IPC, OPERATING SYSTEM PACKAGE, MICROSOFT WINDOWS 7 ULTIMATE SP1 X86 FOR SIMATIC IPC227D / IPC277D",368,"TEM",1,"Simatic",0.20499999999999999,0]
["A5E02380761","SIMATIC PC, SPARE PART BUS BOARD 1X PCI, 1X PCI-E X8 (4LANE) FOR SIMATIC RACK PC: IPC647C",116,"TEM",1,"Simatic",0.1,1]
["A5E03123922","SIMATIC IPC, SPARE PART; REPEAR SET CABLE 1X USB CABLE, 1X FRONTFAN ADAPTER, 1X FRONT OPERATING PANEL CABLE 1X SATA-ODD CABLE (DATA&POWER), 1X SATA-CF CABLE (DATA&POWER), 1X SATA-HDD CABLE SET DATA FOR SIMATIC RACK IPC647C",47.300000000000004,"TEM",1,"Simatic",0.1,1]
["A5E03465405","SIMATIC IPC, SPAREPART MAINBOARD WITH MRAM, CORE I3-3217UE, W/O FIELDBUS FOR SIMATIC IPC477D",1523,"TEM",1,"Simatic",0.2,1]
["A5E03808137","SIMATIC IPC, SPAREPART USB CABLE FOR SIMATIC IPC477D",21,"TEM",1,"Simatic",0.01,1]
["A5E30484420","SIMATIC IPC SPARE PART, REDUNDANT POWER SUPPLY 2X 100/240 V AC; FOR SIMATIC RACK IPC547C, IPC547D, IPC547E, IPC647C, IPC647D, IPC847C, IPC847D",525,"TEM",1,"Simatic",4.03,1]
["A5E31851156","SIMATIC IPC, SPARE PART, FRONT LED BOARD FOR SIMATIC RACK PC: IPC647D",60.900000000000006,"TEM",1,"Simatic",0.3,1]
["A5E32648317","SIMATIC PC, SPARE PART; MAINBOARD IPC227D, 1,0 GHZ, 1 GB RAM",533,"TEM",1,"Simatic",0.28199999999999997,1]
["A5E34732547","SIMATIC IPC, SPARE PART; MAINBOARD IPC277E, N2807",431,"TEM",1,"Simatic",0.2,1]
["A5E35601803","SIMATIC IPC, SPARE PART, PCI/PCIE SLOT CONTACT PLATE SET 5X FOR 5 SLOT / 5X FOR 6 SLOT FOR SIMATIC RACK PC: IPC847D",41,"TEM",1,"Simatic",0.08,1]
["A5E36787436","SIMATIC IPC spare part Powersupply_SV Nano V2_27W for IPC2x7D, IPC2x7E",99.800000000000011,"TEM",1,"Simatic",0.4,1]
["6AV21012AA030AC5","SIMATIC WINCC COMFORT POWERPACK WINCC BASIC -> WINCC COMFORT V13 (NO CHANGE OF VERSION) ENGINEERING SOFTWARE IN TIA PORTAL; FLOATING LICENSE; SOFTWARE AND DOCUMENTATION ON DVD; LICENSE KEY ON USB-STICK; CLASS A; ONLY VALID FOR 6AV2100-0AA03-0AA5 OR 6AV2100-0AA03-0AH5",666,"TEM",1,"Simatic",0.1,0]
["6AV21020AA040AS5","SCE Trainer Package HMI WinCC Advanced V14 / WinCC flexible Advanced 2008 Content: SW and documentation on DVD, 6 user-lic. on USB STick, for WinCC Advanced V14/ WinCC flexible Advanced 2008 engineering, runtime, options; 1x Software for 20 STudents (6AV2102-0AA04-0AS7) for educational purposes only",812,"TEM",1,"Simatic",0.3,0]
["6AV21030DA030AA5","SIMATIC WINCC PROFESSIONAL 512 POWERTAGS V13 SP1 ENGINEERING SOFTWARE IN TIA PORTAL; FLOATING LICENSE; SOFTWARE AND DOCUMENTATION ON DVD; LICENSE KEY ON USB-STICK; CLASS A; 6 LANGUAGES: GE,EN,IT,FR,SP,CH; EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64 BIT), WINDOWS 8.1 (64 BIT), WINSRV 2008/2012 R2 (64 BIT); FOR CONFIGURATION OF SIMATIC PANELS, WINCC RUNTIME ADVANCED, WINCC RUNTIME PROFESSIONAL (UP TO 512 POWERTAGS)",2207,"TEM",1,"Simatic",0.27900000000000003,0]
["6AV21032DH030UC0","SIMATIC WINCC PROFESSIONAL V13 UCL (TIA PORTAL) POWERPACK 512 -> 4096 POWERTAGS V13 FOR ONE INSTALLATION; ENGINEERING-SOFTWARE; SOFTWARE AND DOCU. ON DVD; MASTER LICENSE ON CD; ONLY VALID WITH UCL AGREEMENT",441,"TEM",1,"Simatic",0.1,0]
["6AV21040DA030AH0","SIMATIC WINCC RUNTIME ADVANCED 512 POWERTAGS V13 SP1 RUNTIME SOFTWARE IN TIA PORTAL; SINGLE LICENSE; SOFTWARE, DOCUMENTATION AND LICENSE KEY FOR DOWNLOAD; CLASS A; 6 LANGUAGES: GE,EN,IT,FR,SP,CH; EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64 BIT), WINDOWS 8.1 (64 BIT), WINSRV 2008/2012 R2 (64 BIT) ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY!",1365,"TEM",1,"Simatic",1E-3,0]
["6AV21040FA040AH0","SIMATIC WinCC Runtime Advanced 2048 PowerTags V14, runtime software in TIA Portal; single license; software, documentation and license key for download; class A; 6 languages: GE,EN,IT,FR,ES,ZN; executable under Windows 7 (32 bit, 64 bit), Windows 8.1 (64 bit), WinSrv 2008/2012 R2 (64 bit); ******************************* email address is mandatory for delivery",2100,"TEM",1,"Simatic",1E-3,0]
["6AV21044FF030AE0","SIMATIC WINCC RUNTIME ADVANCED 2048 POWERTAGS V13 SP1, UPGRADE WINCC FLEXIBLE 2008 RUNTIME 2048 POWERTAGS -> WINCC RUNTIME ADVANCED 2048 POWERTAGS V13 SP1; RUNTIME SOFTWARE IN TIA PORTAL; SINGLE LICENSE; SOFTWARE AND DOCUMENTATION ON DVD; LICENSE KEY ON USB-STICK; CLASS A; 6 LANGUAGES: GE,EN,IT,FR,SP,CH; EXECUTABLE UNDER WINDOWS 7 (32 BIT, 64 BIT), WINDOWS 8.1 (64 BIT), WINSRV 2008/2012 R2 (64 BIT)",882,"TEM",1,"Simatic",0.2,0]
["6AV21070RA000BH0","SIMATIC WINCC AUDIT FOR RUNTIME ADVANCED OPTION F. WINCC (TIA PORTAL) LICENSE KEY DOWNLOAD, SINGLE LICENSE F.1 INSTALLATION RT-SW, W/O SW AND DOCU, CLASS A ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY!",714,"TEM",1,"Simatic",1.4999999999999999E-2,0]
["6AV21232DB030AA1","SCHOOL PACKAGE KTP400 BASIC / XB005, CONSISTING OF: 1 X KTP400 BASIC, 1 X SCALANCE XB005 UNMANAGED IE SWITCH, 2 X RJ45 CABLE, LENGTH 6M, 1 X WINCC BASIC (TIA PORTAL) ******************************* FOR EDUCATIONAL PURPOSES ONLY",485,"TEM",1,"Simatic",1.5,0]
["6AV21252AE230AX0","SIMATIC HMI CONNECTION BOX ADVANCED FOR MOBILE PANELS, MOUNTED ON WALL, PROFINET AND PROFISAFE, CONNECTIVITY TO SAFETY RELAIS, LOOP IN OF SAFETY CIRCUIT, CONNECTION POINT RECOGNITION, INTEGRATED SWITCH, MRP-CLIENT, IRT",410,"TEM",1,"Simatic",0.72,1]
["6AV21815AF150AX0","SIMATIC HMI CONNECTING CABLE FOR KTPX00(F) MOBILE, LENGTH 15 METER",252,"TEM",1,"Simatic",1.88,1]
["6AV63722DF060FX4","SIMATIC B.DATA V6.0 SP1 PROFESSIONAL ENERGY DATA MANAGEMENT; UPGRADE 500 TAGS, V5.2/V5.3 -> V6.0 SP1; 1 ACQUISITION COMPONENT, 1 CLIENT, 1 WEB CLIENT, DATA MOBILE, ERP CONNECTION, REPORTING, TRENDER, VISU, MATRIX, KPI, PROFILE; ES/RT-SW; SINGLE LICENSE; LICENSE KEY ON USB STICK; SW AND DOCU ON CD IN GER/EN; EXEC. UNDER  WINDOWS 7 PRO / ULTIMATE (32/64 BIT), WINDOWS 8.1 PRO / ENTERPRISE (64 BIT), WINDOWS SRV 2008 R2 (64 BIT), WINDOWS SRV 2012 R2 (64 BIT)",7350,"TEM",1,"Simatic",0.221,0]
["6AV63722DF270AX0","SIMATIC Energy Manager PRO 3 Web Clients; runtime software; single license; license key on USB STick; without software and documentation",2100,"TEM",1,"Simatic",0.2,0]
["6AV63822EA074AX0","WinCC package for SIMATIC IPC consiSTing of: WinCC RT 2048, V7.4; available only with the same quantity of SIMATIC IPC on the same order form",3374,"TEM",1,"Simatic",0.2,0]
["6AV66118AA000AR0","EPL-MAINTENANCE WINCC FLEXIBLE COMPACT (EPL = ENTERPRISE LICENSE) MAINTENANCE CHARGE F. ROYALTY FOR 12 MONTHS, ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",97.100000000000009,"TEM",1,"Simatic",0.05,0]
["6AV66131DA010AQ0","EPL ROYALTY FOR WINCC FLEXIBLE, 512 POWER TAGS (RT 512) ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",1945,"TEM",1,"Simatic",0.1,0]
["6AV66136AA010AQ0","EPL ROYALTY FOR WINCC FLEXIBLE, CHANGE CONTROL FOR WINCC FLEXIBLE ADVANCED ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",1482,"TEM",1,"Simatic",0.1,0]
["6AV66187ED010AQ0","EPL ROYALTY FOR WINCC FLEXIBLE, ARCHIVES FOR WINCC FLEXIBLE RUNTIME, ONLY VALID COMBINED WITH ENTERPRISE LICENSE CONTRACT, REQUIRES EPL-MASTER",375,"TEM",1,"Simatic",0.1,0]
["6AV66515GA010AA1","STARTER PACKAGE 277 IWLAN V2, COMPRISING: MOBILE PANEL 277 IWLAN V2 WITH HANDWHEEL, KEY SWITCH AND ILLUMINATED PUSHB. UNIT, CHARGING STATION, SPARE BATTERY WINCC FLEXIBLE 2008 STANDARD,",4620,"TEM",1,"Simatic",12.5,0]
["6AV66715CE000AX1","CHARGING STATION FOR MOBILE PANEL 277(F) IWLAN WITH LOCK FOR CHARGE AND HOLD THE MOBILE PANEL 277(F) IWLAN CHARGING OF 2 SPARE BATTERIES",473,"TEM",1,"Simatic",1.9259999999999999,1]
["6XV14404BN20","CONNECTING CABLE PN FOR MOBILE PANELS (PROFINET), SPECIAL LENGTH 20 M",486,"TEM",1,"Simatic",2.48,1]
["6AG10641AA080AA0","COMBI CABLE FOR THE FIRMWARE BOOT FUNCTION A. DRIVEMONITOR (RS 232 C) LENGTH 3 M FOR COMPACTSERVO C3",90.800000000000011,"TEM",1,"Simatic",0.18,1]
["6AG11241QC024AX0","SIPLUS HMI KP1500 COMFORT WITH CONFORMAL COATING BASED ON 6AV2124-1QC02-0AX0 . KEY OPERATION, 15\" WIDESCREEN-TFT-DISPLAY, 16 MIL. COLORS, PROFINET INTERFACE, MPI/PROFIBUS DP INTERFACE, 24 MB USER MEMORY,",5135,"TEM",1,"Simatic",7.32,1]
["6AG11344LB022AB0","SIPLUS ET200S EM 2AI HF -25 ... +60 DEGREES C WITH CONFORMAL COATING BASED ON 6ES7134-4LB02-0AB0 . 2 AI U HIGH FEATURE FOR ET 200S, 15 MM WIDE, CYCLE TIME PER MODULE: 0.5MS, +/-10V; 15 BI + SIGN, +/-5V;15BIT+SIGN, 1..5V; 15BIT, OPERATIONAL LIMITS +/-0.1% WITH LED SF (GROUP FAULT).",383,"TEM",1,"Simatic",5.6000000000000001E-2,1]
["6AG11511AA067AB0","SIPLUS ET 200S IM 151-1 STandard -25...+70Â°C with conformal coating based on 6ES7151-1AA06-0AB0 . Interface module incl. Terminating module Data volume 244byte for each Input and output; max. of 63 Peripheriemodules PROFIBUS DP V0 and V1 up to 2M with connectable; Bus Interfacing via 9-WAY SUB-D",592,"TEM",1,"Simatic",1E-3,1]
["6AG11934CL307AA0","SIPLUS ET200S TM-E15C24-AT 0 ... +70 DEGREES C WITH CONFORMAL COATING BASED ON 6ES7193-4CL30-0AA0 . FOR ELECTRONIC MODULES 2 AI TC HIGH FEATURE, WIDTH 15MM, SPRING-LOAD TERMINALS TERMINAL LEAD TO AUX1, AUX1 IN LINE",40.1,"TEM",1,"Simatic",7.0000000000000007E-2,1]
["6AG12121BE404XB0","SIPLUS S7-1200 CPU 1212C AC/DC/RLY FOR MEDIAL STRESS WITH CONFORMAL COATING BASED ON 6ES7212-1BE40-0XB0 . COMPACT CPU, AC/DC/RY, ONBOARD 8 DI 24V DC 6 DO RELAY 0,5A 2 AI 0 - 10V DC, POWER SUPPLY: AC 85 - 264 V AC @ 47 - 63 HZ, PROGRAM/DATA MEMORY: 30 KB",318,"TEM",1,"Simatic",0.38800000000000001,1]
["6AG12221BF322XB0","SIPLUS S7-1200 SM1222 8DQ -25 ... +70 DEGREES C WITH CONFORMAL COATING BASED ON 6ES7222-1BF32-0XB0 . DIGITAL OUTPUT 8 DQ, 24V DC, TRANSISTOR 0.5A",164,"TEM",1,"Simatic",0.18,1]
["6AG12315PF322XB0","SIPLUS S7-1200 SM1231 RTD 8AI - 25 ... +70 DEGREES C WITH CONFORMAL COATING BASED ON 6ES7231-5PF32-0XB0 . ANALOG INPUT, SM 1231RTD, 8 X AI RTD MODULE",666,"TEM",1,"Simatic",0.29599999999999999,1]
["6AG13146CH047AB0","SIPLUS S7-300 CPU314C-2DP FOR MEDIAL STRESS -25 ... +70 DEGREES C BASED ON 6ES7314-6CH04-0AB0 . COMPACT CPU WITH MPI, 24 DI/16 DO, 4AI, 2AO, 1 PT100, 4 FAST COUNTERS (60 KHZ), INTEGRATED DP INTERFACE, INTEGRATED 24V DC POWER SUPPLY, 192 KBYTE WORKING MEMORY, FRONT CONNECTOR (2 X 40PIN) AND MICRO MEMORY CARD REQUIRED",3171,"TEM",1,"Simatic",0.73799999999999999,1]
["6AG13221HH012AA0","SIPLUS S7-300 SM322 - 20POL -40 ... +70 DGR C WITH CONFORMAL COATING CONFORMITY TO EN50155 T1 CAT 1 CL A/B BASED ON 6ES7322-1HH01-0AA0 . DIGITAL OUTPUT OPTICALLY ISOLAT 16DO, RELAY CONTACTS",551,"TEM",1,"Simatic",0.3,1]
["6AG13343BA107AA0","SIPLUS PS PSU200M 10A -25 ... +70 GRD C WITH CONFORMAL COATING BASED ON 6EP1334-3BA10 . STABILIZED POWER SUPPLY INPUT:120/230-500 V AC OUTPUT: 24 V/10 A DC",471,"TEM",1,"Simatic",0.8,1]
["6AG14143EM077AB0","SIPLUS S7-400 CPU 414-3 PN/DP -25 ... +70 Degrees C with conformal coating Based on 6ES7414-3EM07-0AB0 . Central Processing unit with: 4 MB Working Memory, (2 MB KB Code, 2 MB Data), Interfaces: 1. IF MPI/DP 12 MBIT/S (X1), 2. IF ETHERNET/PROFINET (X5), 3. IF IF964-DP pluggable (IF1)",7917,"TEM",1,"Simatic",0.83599999999999997,1]
["6AG14402AD345FA1","SIPLUS MM440 FS F 45KW FOR MEDIAL STRESS WITH CONFORMAL COATING BASED ON 6SE6440-2AD34-5FA1",11130,"TEM",1,"Simatic",1E-3,1]
["6AG15225EH007AB0","SIPLUS S7-1500 DQ 16x48VUC/125V -40 ... +70 DEG C STARTUP -25 DEG C WITH CONFORMAL COATING BASED ON 6ES7522-5EH00-0AB0 . DQ16 X 24...48VUC/125VDC/0.5A; 16 CHANNELS IN GROUPS OF 1, 0.5A PER GROUP; SUBSTITUTE VALUE; PLEASE NOTE DERATING",1376,"TEM",1,"Simatic",0.2,1]
["6AG16545CQ007XF0","SIPLUS PCS 7 CPU 410-5H BUNDLE -25 ... +70 DEGREES C WITH CONFORMAL COATING BAED ON 6ES7654-5CQ00-0XF0 . PROCESS AUTOMATION FOR S7-400 AND S7-400H WITH SYSTEM EXPANSION CARD MORE THAN 2000 PROCESS OBJECTS . NOT FUER SAFETY APPLICATIONS AL",28875,"TEM",1,"Simatic",1E-3,0]
["6AG22231BH321XB0","SIPLUS S7-1200 SM1223 8DI/8DQ RAIL FOR RAIL APPLICATIONS (EN50155) -25 ... +70 DEGREE C WITH CONFORMAL COATING BASED ON 6ES7223-1BH32-0XB0 . DIGITAL I/O SM 1223, 8 DI / 8 DQ, 8 DI DC 24 V, SINK/SOURCE, 8 DO, TRANSISTOR 0,5A",357,"TEM",1,"Simatic",0.21,1]
["7KG61012EK10","SIMEAS TRANSDUCER (G)MUU FOR ALTERNATING VOLTAGE IN HOUSING, FOR SNAPPING ON MOUNTING RAIL RATED FREQUENCY 50HZ INPUT VOLTAGE AC 100V OUTPUT SIGNAL DC 0 TO 20MA MEASURING RANGE: 0 TO UEN",204,"TEM",1,"Simatic",0.28000000000000003,0]
["7KG61062EK170B","SIMEAS TRANSDUCER (G)MUU FOR ALTERNATING VOLTAGE IN HOUSING, FOR SNAPPING ON MOUNTING RAIL RATED FREQUENCY 50HZ INPUT VOLTAGE AC 100V OUTPUT SIGNAL DC 0 TO 20MA MEASURING RANGE ZERO = SIGNAL RANGE ZERO POWER SUPPLY AC 45 TO 65 HZ, 230V MEASURING RANGE LINEAR 0 TO UEN",550,"TEM",1,"Simatic",0.33,0]
["7KG61062SN270B","SIMEAS TRANSDUCER (G)MUU FOR ALTERNATING VOLTAGE IN HOUSING, FOR SNAPPING ON MOUNTING RAIL RATED FREQUENCY 50HZ INPUT VOLTAGE AC 500V OUTPUT SIGNAL DC 4 TO 20MA (LIVE ZERO) POWER SUPPLY AC 45 TO 65 HZ, 230V MEASURING RANGE LINEAR 0 TO UEN",590,"TEM",1,"Simatic",0.33,0]
["7KG61112GK10","SIMEAS TRANSDUCER (G)MUI FOR ALTERNATING CURRENT IN HOUSING, FOR SNAPPING ON MOUNTING RAIL RATED FREQUENCY 50HZ NOMINAL INPUT CURRENT 7,5A OUTPUT SIGNAL DC 0 TO 20MA",204,"TEM",1,"Simatic",0.28000000000000003,0]
["7KG61132FN240B","SIMEAS TRANSDUCER (G)MUI FOR ALTERNATING CURRENT IN HOUSING, FOR SNAPPING ON MOUNTING RAIL RATED FREQUENCY 50HZ INPUT CURRENT 6A OUTPUT SIGNAL DC 4 TO 20MA (LIVE ZERO) POWER SUPPLY DC 88 - 264V MEASURING RANGE LINEAR 0 TO IEN",590,"TEM",1,"Simatic",0.33,0]
["7KG61311KM11","SIMEAS-T TRANSDUCER FOR DC-VOLTAGE AND CURRENT & ISOLATING AMPLIFIERS INPUT CURRENT: -20MA TO 20MA DC OUTPUT SIGNAL RANGE: -10V TO 10V DC ZERO POSITION: INPUT: 0MA,V = OUTPUT: 0MA,V AUXILIARY POWER SUPPLY: 19,2 TO 72V DC",816,"TEM",1,"Simatic",0.33,0]
["7KG61311XN21","SIMEAS-T TRANSDUCER FOR DC-VOLTAGE AND CURRENT & ISOLATING AMPLIFIERS INPUT VOLTAGE: -30V TO 30V DC OUTPUT SIGNAL RANGE: 4MA BIS 20MA DC (LIVE ZERO) ZERO POSITION: INPUT: 0MA,V = OUTPUT: 4MA AUXILIARY POWER SUPPLY: 19,2 TO 72V DC",816,"TEM",1,"Simatic",0.33,0]
["6GF34001AP032AA0","ACTION PACK PAT-GENIUS; FOR MV440 CODE READERS; SINGLE LICENSE, EXTENDS ABOVE DEVICES BY FUNCTIONALITY FOR OBJECT RECOGNITION AND CHECK; DELIVERED ON USB STICK; VIA ALM LOADABLE ON DEVICE; PREREQUISITE: FW > V6.0",652,"TEM",1,"Simatic",0.2,0]
["6GF90011AP02","CS-MOUNT TO C-MOUNT ADAPT. RING 5MM",22.8,"TEM",1,"Simatic",7.0000000000000007E-2,1]
["6GK15003AA10","PROFIBUS OBT OPT. BUS TERMINAL  FOR CONNECT. A PROFIBUS CLIENT WITHOUT INTEGRATED  OPT.  INTERFACE TO OPTICAL  PROFIBUS DP, WITHOUT SIMPLEX CONNECTOR",252,"TEM",1,"Simatic",0.255,1]
["6GK17000AA130AA0","SIMATIC NET SOFTWARE DVD PC/WINDOWS V13; TRIAL 14 DAYS LICENSE FOR 1 INSTALLATION R-SW, SW ON DVD, CLASS A; WITH ELECTR. MANUAL ON  DVD; 2 LANGUAGES (G,E); FOR 32/64BIT: WIN 7 SP1 PROF/ULT, 64BIT: WIN 8.1 PRO; WINDOWS 10, SERVER 2008 R2 SP1, 2012 R2",79.2,"TEM",1,"Simatic",0.34300000000000003,0]
["6GK17041HW120AA0","SIMATIC NET SOFTN.-IE PNIO V12 SW F.S7-,PN IO CONTROLLER; COMM.,OPC,PG/OP-COMM.,CONF. SW; SINGLE LICENSE F.1 INSTALLAT. ; R-SW, SW + ELECTR. MAN ON  DVD; LICENSE KEY ON USB-STICK, CLASS A; 2-LANGUAGES (G,E); FOR 32/64BIT: WIN 7 SP1 PROF/ULT, WIN 8.1 PROF; 64BIT: WINDOWS SERVER 2008 R2 SP1, 2012 R2",830,"TEM",1,"Simatic",0.32200000000000001,0]
["6GK17041PW713AA0","SIMATIC NET IE SOFTNET-PG/2008 SW F. PG/OP-COMM. SINGLE LICENSE F.1 INSTALLATION R-SW, SW + ELECTR. MAN ON CD, LICENSE KEY ON USB-STICK, CLASS A 2-LANGUAGES (G,E); FOR 32BIT: WIN XP PROFESSIONAL; WIN VISTA ULTIMATE/BUSINESS; WIN 2003/2008 SERVER; FOR CP1612",541,"TEM",1,"Simatic",0.35099999999999998,0]
["6GK17045SW130AA0","SIMATIC NET SOFTNET-PB DP-SLAVE V13; SW FOR DP-SLAVE WITH OPC-SERVER AND PROJ.-SW; SINGLE LICENSE F.1 INSTALLATION R-SW, SW+ELECTR. MAN ON  DVD; LICENSE KEY ON USB-STICK, CLASS A; 2 LANGUAGES (G,E); FOR 32/64BIT: WIN 7 SP1 PROF/ULT, 64BIT: WIN 8.1 PRO; WINDOWS 10, SERVER 2008 R2 SP1, 2012 R2 FOR CP5612/CP5622/CP5711",216,"TEM",1,"Simatic",0.33500000000000002,0]
["6GK17061NX120AA0","SIMATIC NET IE SNMP OPC-SERVER EXTENDED V12;ADMIN. OF UP TO 200 IP-ADR.;INCL. MIB-COMPILER; SINGLE LICENSE F.1 INSTALLATION R-SW, SW + ELECTR. MAN ON DVD; LICENSE KEY ON USB-STICK, CLASS A; 2-LANGUAGES (G,E);FOR 32/64BIT: WIN 7 SP1 PROF/ULT, WIN 8.1 PROF; 64BIT: WINDOWS SERVER 2008 R2 SP1, 2012 R2 FOR CP1613/ CP1623 CP1612 (NO WIN 8.1, SRV2012R2)",1565,"TEM",1,"Simatic",0.23200000000000001,0]
["6GK17135DB643AA0","SIMATIC NET PB DP-5613/2006 SW FOR DP-COMM., INCL. PG, FDL OPC-SERVER AND NCM PC; SINGLE LICENSE F.1 INSTALLATION R-SW, SW + ELECTR. MAN. ON CD LICENSE KEY ON FD,CLASS A 2-LANGUAGE (G,E), FOR 32BIT WINDOWS XP PRO, 2000PRO/SV; WIN 2003 SERVER; FOR CP5613/ CP5614, EL/FO",410,"TEM",1,"Simatic",0.36399999999999999,0]
["6GK17811JA130AA0","SINEMA SERVER 250 V13+SP1 DELIVERED ON  DVD MONITORING FOR INDUSTRIAL NETWORKS INCL PROFINET AUTOMATIC INVENTORY DETERMINATION OF TOPOLOGY CONTINUOUS DIAGNOSIS REPORTING, STATISTICS, ALARMS ADAPTABLE DEVICE PROFILES CAPABLE OF BEEING INTEGR IN HMI WEBSERVER-WEBCLIENT ARCHITECT. LICENSE TYPE SINGLE MONITORABLE IP UNITS 250 WINDOWS 7 SP1 64BIT WINDOWS SERVER 2008 R2+SP1",3234,"TEM",1,"Simatic",0.15,0]
["6GK19001LP000AB0","FC FO SC COUPLER ON-SITE MOUNTING ON FC FO CABLES (62.5/200/230) PACKAGE: 5 PCS. DUPLEX COUPLER",305,"ΠΑΚ",1,"Simatic",0.08,0]
["6GK19011BE000AA1","INDUSTRIAL ETHERNET FASTCONNECT RJ45 MODULAR OUTLET,BASE MODULE WITH 2FE INSERT, REPL. INSERT FOR 2 X 100 MBIT/S INTERFACE",61.300000000000004,"TEM",1,"Simatic",0.4,0]
["6GK19050FA00","7/8\" CONNECTING PLUG W. AXIAL CABLE OUTLET FOR FIELD ASSEMBLY OF ET 200; PIN CONNECTOR, PACK. UNIT 5 PIECES",105,"ΠΑΚ",1,"Simatic",0.26500000000000001,0]
["6GK50041BF001AB2","SCALANCE XB004-1LD UNMANAGED INDUSTRIAL ETHERNET SWITCH FOR 10/100MBIT/S; WITH 4 X 10/100MBIT/S TWISTED PAIR- PORTS WITH  RJ45-SOCKETS; 1 X100MBIT/S SINGLEMODE GLASS FOC-PORT WITH SC-SOCKET; FOR CONFIGURING SMALL STAR- AND LINE TOPOGRAPHIES; LED-DIAGNOSIS, IP20, 24 V DC POWER SUPPLY, MANUAL AVAILABLE AS DOWNLOAD",300,"TEM",1,"Simatic",0.251,1]
["6GK52040BS003PA3","SCALANCE X204RNA EEC; REDUNDANT NETWORK ACCESS; FOR PRP AND HSR NETWORKS; 2 X 100MBIT/S RJ45 PORTS; 2 X 100MBIT/S COMBO-PORTS; LED-DIAGNOSIS; FAULT SIGNAL- CONTACT AND SET BUTTON; REDUNDANT POWER SUPPLY; NETWORK-MANAGEMENT; INCL. ELECTRONIC MAN ON CD C-PLUG OPTIONAL",909,"TEM",1,"Simatic",1.244,1]
["6GK52133BF002TB2","SCALANCE XB213-3LD MANAGEABLE LAYER 2 IE-SWITCH 13X 10/100 MBITS/S RJ45 PORTS 3X SM FO SC-PORT 1X CONSOLE PORT DIAGNOSTICS LED REDUNDANT POWER SUPPLY STP. RANGE 0 DGR C UP TO +60 DGR C; DIN-RAIL MOUNTING ETHERNET/IP CONFORMAL DEFAULT ETHERNET/IP",1565,"TEM",1,"Simatic",0.57299999999999995,1]
["6GK53203BF002AA3","SCALANCE X320-3LDFE MANAGED  IE SWITCH, 20 X 10/100 MBIT/S RJ45 PORTS, 1 X 100MBIT/S SC PORT MM 2 X 100MBIT/S SC PORT SM LED-DIAGNOSTICS, FAULT SIGNAL CONTACT WITH SELECT/ SET BUTTON, PROFINET-IO DEVICE, NETWORK- MANAGEMENT, INTEGRATED REDUNDANCY MANAGER OFFICE FEATURES (RTEMP, VLAN, IGMP,..) C-PLUG IN THE SCOPE OF SUPPLY",3917,"TEM",1,"Simatic",1.8660000000000001,1]
["6GK55248GS003AR2","SCALANCE XR524-8C; MANAGED IE SWITCH; LAYER 3 AVAILABLE W. KEY-PLUG; POWER SUPPLY 230V AC; 24 X 10/100/1000 MBIT/S RJ45; 8 X 100/1000 MBIT/S SFP; CONTAINS 8 COMBO PORTS; 24 PORTS CAN BE USED IN TOTAL; FAULT-SIGNAL CONTACT; SELECT/SET-BUTTON; PROFINET-IO DEVICE; REDUNDANCY FUNCTIONS; OFFICE FEATURES (RTEMP, VLAN, IGMP,..); C-PLUG IN SCOPE OF SUPPLY",4620,"TEM",1,"Simatic",5.16,1]
["6GK57481FC000AA0","IWLAN Client, SCALANCE W748-1 RJ45, 1 radio, 3 R-SMA antenna connector, iFeatures support via KEY-PLUG, IEEE 802.11a/b/g/h/n, 2,4/5GHz, brutto 450 MBit/s per radio, 1x RJ45 max. 1 Gbit/s, PoE, redundant DC 24 V, term. block, IP30, Temp: -20 ...+60Â°C, WPA2/802.11i/e, signal contact Note national approvals! CERT ID: RAPN-W1-RJ-E3, contains: MPCIE-R1-ABGN-U3, scope of supply: manuals on CD, German/English, 2x terminal block; for use outside USA/Israel",704,"TEM",1,"Simatic",1.907,1]
["6GK57912DC000AA0","Power-Supply PS 791-2DC, DC/DC power supply 10 W, IP65 -40...+70Â° C, Input: DC 12...24V, Output: DC 18 V, usable only in combination with SCALANCE W-786; scope of supply: manual, German/English",205,"TEM",1,"Simatic",0.308,1]
["6GK57980PT002AA0","SIMATIC N-CONNECT/SMA FEMALE/ FEMALE PANEL FEEDTHROUGH 2.4 GHZ AND 5 GHZ CABINET CABLE DUCT FOR MAXIMAL WALL THICKNESS 5.5 MM",16.2,"TEM",1,"Simatic",3.5000000000000003E-2,0]
["6GK59070PA00","KEY-PLUG W700 Security, replaceable medium for activating security features f. SCALANCE W700 Access Points, allows simple device exchange in case of failure and recording configuration data;",210,"TEM",1,"Simatic",2.5000000000000001E-2,1]
["6GK59912AH008AA0","SCALANCE X ACCESSORIES; MEDIA MODULE MM991-2P; 2 X 100MBIT/S;  SC RJ POF/PCF- PORTS; OPTICAL POF UP TO MAX. 50 M; PCF UP TO MAX 100 M;",378,"TEM",1,"Simatic",0.121,1]
["6GK75426UX000XE0","COMMUNICATION PROCESSOR",473,"TEM",1,"Simatic",0.20100000000000001,1]
["6GK75431AX000XE0","COMMUNICATION PROCESSOR CP 1543-1 FOR CONNECTING SIMATIC S7-1500 TO INDUSTRIAL ETHERNET: TCP/IP, ISO, UDP, S7- COMMUNICATION, IP-BROADCAST/ MULTICAST, SECURITY (HARDWARE- IDENTIFICATION, IP/MAC ACCESS LIST, FIREWALL), DIAGNOSIS SNMPV1/V3, DHCP, FTP CLIENT/ SERVER, E-MAIL, IPV4/IPV6, DATA STORAGE ON SD CARD OF CPU, CLOCK SYNCHRONISATION VIA NTP, ACCESS TO WEBSERVER OF CPU; GIGABIT-SS 1XRJ45 (10/100/1000 MBIT)",1502,"TEM",1,"Simatic",0.1,1]
["6GT23981CD600AX0","RF300 / RF200 ANTENNA ANT 3S FOR CONNECTION TO RF250R AND RF350R IP 64, -25 UP TO +70 DGR/C, DIMENSIONS 50X28X10 MM INCL. ANTENNA CONNECTING CABLE PUR, UL 758, LENGTH 3M TRAILING CAPABILITY CONNECTOR M8 STRAIGTH/M8 FOR TRANSPONDER ANGLED  MDS D117, MDS D127, MDS D421",550,"TEM",1,"Simatic",160.12,1]
["6GT26005AE00","TRANSPONDER MDS D521 FOR RF200 ONLY TOOL PILL IN METAL ISO 15693 CHIP TYPE,FUJITSU MB89R112, 8192 BYTE FRAM USER MEMORY 10 X 4.5 MM (DXH); -25 UP TO +85 DGR; MIN. ORDER QUANTITY 10 STUECK",56.300000000000004,"TEM",1,"Simatic",0.01,10]
["6GT28011AB100AX1","SIMATIC RF300 READER RF310R (RF300+ISO15693) WITH RS422-INTERFACE (3964R) IP 67, -25 UP TO +70 DGR C, 55 X 75 X 30 MM, WITH INTEGRATED ANTENNA SPECIAL VERSION WITH ROTATED BASEPLATE (90 DGR.)",857,"TEM",1,"Simatic",0.14000000000000001,1]
["6GT28102BB800AX1","SIMATIC RF610T SPECIAL VERSION ISO CARD;PVC; 86 X 54 X 0.4 MM ATEX ZONE 2/22 ISO 18000-6C, EPC CLASS 1 GEN 2 FREQUENCY 860 UP TO 928 MHZ CHIP TYPE, NXP G2XM EPC 240 BIT 64 BYTE  ADD-ON MEMORY -25 UP TO +85 DGR/C; MINIMAL ORDER QUANTITY 1000 PCS",165,"TEM",100,"Simatic",3.0000000000000001E-3,0]
["6GT28152BH50","SIMATIC RF600 CONNECT. CABLE ANTENNA L5; PREASSEMBLED, BETWEEN READER AND ANTENNA; IP65; TRAILING (TRAILING CAPABILITY); PE, CMR/MPR, LENGTH 5 M",158,"TEM",1,"Simatic",1,0]
["6GT28900BB20","SIMATIC RF600 ANTENNA ATTENUATOR 10 DB ATTENUATION; 50 OHM; 2 W; CONNECTION R-TNC; FOR ANTENNAS SIMATIC RF600 PACKAGING UNIT 2 PIECES",127,"TEM",1,"Simatic",1,0]
["6NH77010AR","SINAUT ST7, TEST CABLE FOR CONNECTING TWO TIMS VIA THE RS232-INTERFACE WITHOUT INTERCONNECTION OF MODEMS (NULL-MODEM); CABLE LENGTH 6 M",132,"TEM",1,"Simatic",0.16500000000000001,0]
["6NH99100AA210AA0","TELECONTROL SERVER BASIC 8 V3; SINGLE LICENSE FOR 1 INSTAL- LATION; OPC (UA)-SERVER FOR IP-COMMUNICATION W. S7-1200 A. S7-200; CONNECT. MANAGEMENT TO 8 REMOTE STATIONS; ROUTING BETWEEN S7 STATIONS; MULTI PROJECT-CAPABLE; WIRING DIAGNOSTICS;STATION MONITORING; TELESERVICE GATEWAY; IMPORT OF SINAUT MICRO SC PROJECTS; GERMAN AND ENGLISH USER INTERFACE; DOCUMENTATION ON CD IN GERMAN AND ENGLISH,",525,"TEM",1,"Simatic",0.23400000000000001,0]
["6XV18205BH40","SIMATIC NET, FIBER OPTIC CABLE (62.5/125)STANDARD CABLE, SPLITTABLE, PREASSEMBLED WITH 4 BFOC CONNECTORS LENGTH: 4 M",128,"TEM",1,"Simatic",0.314,0]
["6XV18206BT10","SIMATIC NET, FLEXIBLE FIBER OPTIC CABLE (62.5/125), TRAILING CABLE, SPLITTABLE, PREASSEMBLED WITH 4 BFOC CONNECTORS, LENGTH: 100 M",1176,"TEM",1,"Simatic",13.51,0]
["6XV18211CT20","SIMATIC NET, PROFIBUS PCF FIBER OPTIC, WITH 4 PCF SIMPLEX CONNECTORS LENGTH = 200 M",933,"TEM",1,"Simatic",4.5,0]
["6XV18302AN10","SIMATIC NET, CONN. CABLE 830-2 F. PROFIBUS, PREASSEMBLED CABLE WITH 2 SUB-D-CONNECTORS 9-POLE, SWITCHABLE TERMINATING RESISTORS 10 M",131,"TEM",1,"Simatic",0.96399999999999997,0]
["6XV18402AT50","IE FC TP STANDARD CABLE GP 2X2 (PROFINET TYPE A), CAT5E, BUS CABLE 4-WIRE, SHIELDED, SPEC. DESIGN FOR RAPID INSTALL. AN IE FC RJ45 PLUG 2X2, 500 M",767,"TEM",1,"Simatic",30.5,0]
["6XV18500CH20","SIMATIC NET, ITP XP STANDARD CABLE 9/9 FOR INDUSTR. ETHERNET ITP STANDARD CABLE,PREASSEMBLED WITH 2 X 9-PIN  ITP CONNECTORS, FOR CASCADING OF ACTIVE ITP NETWORK COMPONENTS, LENGTH: 2 M",76.3,"TEM",1,"Simatic",0.30299999999999999,0]
["6XV18603PH30","SIMATIC NET, PROFIBUS ECOFAST HYBRID CABLE GP, 2XCU 0.64 MM, 4XCU 1.5 SQMM, CABLE PREASSEMBLED WITH ECOFAST CONNECTOR AND SOCKET, TRAILING TYPE, LENGTH 3 M",75.5,"TEM",1,"Simatic",0.75,0]
["6XV18603PN20","SIMATIC NET, PROFIBUS ECOFAST HYBRID CABLE GP, 2XCU 0.64 MM, 4XCU 1.5 SQMM, CABLE PREASSEMBLED WITH ECOFAST CONNECTOR AND SOCKET, TRAILING TYPE, LENGTH 20 M",189,"TEM",1,"Simatic",3.18,0]
["6XV18703RH60","SIMATIC NET INDUSTRIAL ETHERNET TP XP CORD RJ45/RJ45, CAT 6A, CROSSED TP CABLE 4X2, PREASSEMBLED W. 2 RJ45 CONNECTORS, LENGTH 6 M",28.400000000000002,"TEM",1,"Simatic",0.22500000000000001,0]
["6XV18733AH50","SIMATIC NET FO STANDARD CABLE 50/125, PREASSEMBLED WITH 2X2 BFOC CONNECTORS, LENGTH 5.0 M",68.900000000000006,"TEM",1,"Simatic",0.22,0]
["6XV18735RN50","SIMATIC NET FO ROBUST CABLE GP 50/125, PREASSEMBLED WITH 2 X LC DUPLEX CONNECTORS, LENGTH 50 M",378,"TEM",1,"Simatic",3,0]
["6XV18736GT20","SIMATIC NET FO GROUND CABLE 50/ 125, PREASSEMBLED WITH 2X2 SC CONNECTORS, INSERTION GUIDE, LENGTH 200 M",1344,"TEM",1,"Simatic",18.02,0]
["6XV18815AH30","IE ROBUST CONNECTING CABLE M12-180/M12-180, IP69, PREASS. IE FC ROBUST FOOD CABLE GP 2X2, W. 2 M12 CONNECTORS (D-CODED), LENGTH 3.0 M",53.6,"TEM",1,"Simatic",0.26,0]
["6EP13232BA10","SITOP PSU100B 12 V/10 A STABILIZED POWER SUPPLY INPUT: 120/230 V AC OUTPUT: 12 V/10 A DC",217,"TEM",1,"Simatic",0.7,1]
["6EP13342AA010AB0","SITOP SMART 240 W STABILIZED POWER SUPPLY INPUT: 120/230 V AC OUTPUT: 24 V DC/10 A VERSION FOR WALL MOUNTING",182,"TEM",1,"Simatic",0.85,1]
["6EP19312FC21","SITOP DC USV MODULE 24 V/40 A UNINTERRUPTIBLE POWER SUPPLY WITHOUT INTERFACE INPUT: 24 V DC/43 A OUTPUT: 24 V DC/40 A",331,"TEM",1,"Simatic",1.1000000000000001,1]
["6EP19711BA00","SIMATIC S7-300, INSTALLATION ADAPTER FOR SNAPPING THE PS307 ONTO THE DIN RAIL 35X15/7,5 MM SUITABLE FOR 6ES7307-1BA01*, -1EA01*, -1KA02* AND LATER",16.900000000000002,"TEM",1,"Simatic",0.03,1]
["6ES73071KA020AA0","SIMATIC S7-300 STABILIZED POWER SUPPLY PS307 INPUT: 120/230 V AC OUTPUT: DC 24 V DC/10 A",192,"TEM",1,"Simatic",0.8,1]
["6ES79223BC500AF0","FRONT CONNECT. F.SIMATIC S7-300 20POL. (6ES7921-3AH00-0AA0) W. 20 SINGLE CORES 0.5 MM2, H05V-K SINGLE CORES, CRIMP-TYPE VERSION PACK. UNIT=1 PCS. L = 2.5 M",49.400000000000006,"TEM",1,"Simatic",0.63400000000000001,0]
["6ES79223BJ000AU0","CABLE WITH FRONT CONNECTOR FOR SIMATIC S7-300 20PIN (6ES7392-1AJ00-0AA0) TO 50PIN D-SUB FEMALE FOR ET200M; 0.50 MM2 LENGTH 8M",195,"TEM",1,"Simatic",2.2160000000000002,0]
["6ES79225BG500UC0","FRONT CONN. F. SIMATIC S7-1500 40-PIN (6ES7592-1AM00-0XB0) W. 40 SINGLE CORES 0.5 MM2 CORE-TYPE UL/SCA CERTIFIED SCREW-TYPE VERSION L = 6.5M",132,"TEM",1,"Simatic",2.77,0]
["6ES79230CG000BA0","TWISTED RIBBON CABLE WITH 16 CORES 0.14 MM2, LENGTH: 60 M, SHIELDED",270,"TEM",1,"Simatic",8.8000000000000007,0]
["6ES79242CC200AC0","TERMINAL BLOCK TPA 3-TIER FOR ANALOG MODULES OF SIMATIC S7-1500 SORT: PUSH-IN TERMINAL WITHOUT LED, PACK. UNIT=1PCS 50 POLE IDC CONNECT. F. CABLE",78.800000000000011,"TEM",1,"Simatic",0.27,0]
["6ES74001JA010AA0","SIMATIC S7-400, UR2 RACK, CENTRALIZED AND DISTRIBUTED WITH 9 SLOTS 2 REDUNDANT PS PLUGGABLE",461,"TEM",1,"Simatic",2.456,1]
["6ES74163FS070AB0","SIMATIC S7-400, CPU416F-3 PN/DP CENTRAL PROCESSING UNIT WITH: 16 MB WORKING MEMORY, (8 MB KB CODE, 8 MB DATA), INTERFACES: 1. IF MPI/DP 12 MBIT/S (X1), 2. IF ETHERNET/PROFINET (X5), 3. IF IF964-DP PLUGABLE (IF1)",12134,"TEM",1,"Simatic",1.069,1]
["6ES74613AA007AA0","SIMATIC S7-400, TERMINATOR FOR RECEIVER IM461-3 INTERFACE MOD.",88.2,"TEM",1,"Simatic",7.0999999999999994E-2,1]
["6ES74921CL001AB0","SIMATIC S7-400, FRONT CONNECTOR FOR SIGNAL MODULES, FOR CRIMP SNAP-IN CONTACT, 48-POLE 84 PIECES PER PACKAGING UNIT",2085,"ΠΑΚ",1,"Simatic",11.54,0]
["6AV21050BA040AA0","SIMATIC WINCC RT PROFESSIONAL, 128 POWERTAGS V14, RUNTIME SW IN THE TIA PORTAL, SINGLE LICENSE, SW AND DOCUMENTATION ON DVD, LICENSE KEY ON USB STICK, CLASS A, 6 LANG. (DE,EN,IT,FR,SP,CH), EXECUTABLE UNDER WINDOWS 7 PROF/ENT/ULT +SP1 (32 BIT)/ 7 PROF/ENT/ULT +SP1 (64 BIT)/ 8.1 PRO/ENT (64 BIT)/ SERVER2008 R2 +SP1 (64 BIT)/ SERVER 2012 R2 (64 BIT)",2371,"TEM",1,"Simatic",0.1,0]
["6AV21050RA030AA0","SIMATIC WINCC RT PROFESSIONAL, 153600 POWERTAGS V13 SP1, RUNTIME SW IN THE TIA PORTAL, SINGLE LICENSE, SW AND DOCUMENTATION ON DVD, LICENSE KEY ON USB STICK, CLASS A, 6 LANGUAGES(GE,EN,IT,FR,SP,CH), EXECUTABLE UNDER WINDOWS 7 PROF/ENT/ULT +SP1 (32 BIT)/ 7 PROF/ENT/ULT +SP1 (64 BIT)/ 8.1 STD/PROF/ENT/ULT (64 BIT)/ SERVER2008 R2 +SP1 (64 BIT)/ SERVER 2012 (64 BIT)",12128,"TEM",1,"Simatic",0.2,0]
["6AV21052FF040AC0","SIMATIC WINCC RT PROFESSIONAL, POWERPACK RT ADVANCED 2048 -> RT PROF 2048 POWERTAGS V14 (NO CHANGE OF VERSION) RUNTIME-SW IN THE TIA PORTAL, SINGLE LICENSE, SW AND DOCUMENTATION ON DVD, LICENSE KEY ON USB STICK, CLASS A, 6 LANGUAGES(GE,EN,IT,FR,SP,CH), EXECUTABLE UNDER WINDOWS 7 PROF/ENT/ULT +SP1 (32 BIT)/ 7 PROF/ENT/ULT +SP1 (64 BIT)/ 8.1 PRO/ENT (64 BIT)/ SERVER2008 R2 +SP1 (64 BIT)/ SERVER 2012 R2 (64 BIT)",2244,"TEM",1,"Simatic",0.1,0]
["6AV21053FF020AE0","WINCC RUNTIME PROFESSIONAL 2048  POWERTAGS V12 SP1, UPGRADE V11 -> V12 SP1, RUNTIME-SW, SINGLE LICENSE SW AND DOCUMENTATION ON DVD, LICENSE KEY ON USB STICK, CLASS A, 6 LANGUAGES(GE,EN,IT,FR,SP,CH), EXECUTABLE UNDER WINDOWS XP (32 BIT) / WINDOWS 7 (32/64 BIT) / WINSRV 2003 R2/2008 (32 BIT) / WINSRV 2008 R2 (64 BIT)",1159,"TEM",1,"Simatic",0.41099999999999998,0]
["6AV21054BB030AE0","SIMATIC WINCC RT PROF V13 SP1, UPGRADE WINCC V7.0/7.2 RT 128 POWERTAGS -> WINCC RT PROFESSIONAL 128 POWERTAGS V13 SP1, RUNTIME-SW IN THE TIA PORTAL, SINGLE LICENSE, SW AND DOCUMENTATION ON DVD, LICENSE KEY ON USB STICK, CLASS A, 6 LANGUAGES(GE,EN,IT,FR,SP,CH), EXECUTABLE UNDER WINDOWS 7 PROF/ENT/ULT +SP1 (32 BIT)/ 7 PROF/ENT/ULT +SP1 (64 BIT)/ 8.1 STD/PROF/ENT/ULT (64 BIT)/ SERVER2008 R2 +SP1 (64 BIT)/ SERVER 2012 (64 BIT)",949,"TEM",1,"Simatic",0.2,0]
["6AV21054RR030AE0","SIMATIC WINCC RT PROF V13 SP1, UPGRADE WINCC V7.0/7.2 RT 153600 POWERTAGS -> WINCC RT PROFESSIONAL 153600 POWERTAGS V13 SP1, RUNTIME-SW IN THE TIA PORTAL, SINGLE LICENSE, SW AND DOCUMENTATION ON DVD, LICENSE KEY ON USB STICK, CLASS A, 6 LANGUAGES(GE,EN,IT,FR,SP,CH), EXECUTABLE UNDER WINDOWS 7 PROF/ENT/ULT +SP1 (32 BIT)/ 7 PROF/ENT/ULT +SP1 (64 BIT)/ 8.1 STD/PROF/ENT/ULT (64 BIT)/ SERVER2008 R2 +SP1 (64 BIT)/ SERVER 2012 (64 BIT)",4499,"TEM",1,"Simatic",0.2,0]
["6AV21070KT000BH0","SIMATIC WINCC WEBDIAGNOSTICS CLIENT FOR RUNTIME PROFESSIONAL OPTION F. WINCC (TIA PORTAL) LICENSE KEY DOWNLOAD, SINGLE LICENSE F.1 INSTALLATION RT-SW, W/O SW AND DOCU, CLASS A ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY!",2379,"TEM",1,"Simatic",1.4999999999999999E-2,0]
["6AV21072KM000BJ0","SIMATIC WINCC WEBNAVIGATOR FOR RUNTIME PROFESSIONAL POWERACK 50 -> 100 CLIENTS OPTION F. WINCC (TIA PORTAL) LICENSE KEY DOWNLOAD, SINGLE LICENSE F.1 INSTALLATION RT-SW, W/O SW AND DOCU, CLASS A ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY!",15183,"TEM",1,"Simatic",1.4999999999999999E-2,0]
["6AV21152FA030AA0","WINCC RUNTIME PROFESSIONAL SW PACKAGE FOR SIMATIC IPC 2048 POWERTAGS, CONTAINS: WINCC RUNTIME PROF. 2048 POWERTAGS V13, AVAILABLE ONLY W. SAME QTY OF SIMATIC IPC ON SAME ORDER FORM",3599,"TEM",1,"Simatic",0.2,0]
["6AV63621BA000BB0","WINCC/WEB NAVIGATOR, DIAGNOSTIC CLIENT LICENSE, OPTION F. WINCC AS OF V7.4 AND WINCC PROF. AS OF V14, RUNTIME-SW, SINGLE LICENSE, LICENSE KEY ON USB STICK",3262,"TEM",1,"Simatic",0.14799999999999999,0]
["6AV63622AJ000AH0","WINCC/WEBUX MONITOR, 30 CLIENT LICENSES (COUNTABLE), OPTION F. WINCC AS OF V7.3 AND WINCC PROF. AS OF V14, RUNTIME-SW, SINGLE LICENSE, LICENSE KEY DOWNLOAD, ON SERVER SIDE WINDOWS 64 BIT REQUIRED ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY!",8610,"TEM",1,"Simatic",1E-3,0]
["6AV63711CB074AX0","WINCC/USER ARCHIVES V7.4, OPTION F. WINCC V7.4, RUNTIME-SW, SINGLE LICENSE, LICENSE KEY ON USB STICK",816,"TEM",1,"Simatic",0.14099999999999999,0]
["6AV63711DN072LA0","WINCC/DATAMONITOR V7.2, POWERPACK FROM 1 TO 3 CLIENTS, SINGLE LICENSE, LICENSE KEY ON USB STICK",1160,"TEM",1,"Simatic",0.1,0]
["6AV63711DQ173BC0","WINCC ARCHIVE POWERPACK V7.3 UPGRADING FROM 5000 TO 10000 ARCHIVE TAGS, FOR SIMATIC WINCC V7.3, RUNTIME SW, SINGLE LICENSE, COUNT RELEVANT",4836,"TEM",1,"Simatic",0.2,0]
["6AV63711DX070AX0","WINCC/INDUSTRIALDATABRIDGE V7.0 SP3, DATA EXCHANGE W. DATA BASES AND OPC SERVERS  (G/E/F/I/S), 128 TAGS, OPTION F. WINCC V7.0 SP3, RUNTIME-SW, SINGLE LICENSE EXECUTABLE UNDER WINXPPROF",1182,"TEM",1,"Simatic",0.24,0]
["6AV63711HF073AX0","WINCC/REDUNDANCY V7.3, OPTION FOR SIMATIC WINCC V7.3, RUNTIME SOFTWARE, SINGLE LIC. F. 2 INSTALLATIONEN LICENSE KEY DOWNLOAD ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY!",3431,"TEM",1,"Simatic",1E-3,0]
["6AV63711HV073AX0","WINCC/AUDIT RT V7.3, FOR EACH OPERATOR STATION, GENERATION OF AUDIT-TRAIL, OPTION FOR WINCC V7.3, RUNTIME-SW, SINGLE LICENSE SW AND LICENSE KEY DOWNLOAD ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY!",766,"TEM",1,"Simatic",1E-3,0]
["6AV63711JQ173BC0","WINCC ARCHIVE POWERPACK V7.3 UPGRADING FROM 5000 TO 10000 ARCHIVE TAGS, FOR SIMATIC WINCC V7.3, RUNTIME SW, SINGLE LICENSE, COUNT RELEVANT LICENSE KEY DOWNLOAD ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY!",4836,"TEM",1,"Simatic",1E-3,0]
["6AV63712BD073AX0","WINCC POWERPACK RT 128/512 FOR SIMATIC WINCC V7.3, RT LICENSE W/O VERSION CONVERSION FROM 128 TO 512 POWER TAGS, SINGLE LICENSE",1277,"TEM",1,"Simatic",0.15,0]
["6AV63712BG073AX0","WINCC POWERPACK RT 512/2048 FOR SIMATIC WINCC V7.3, RT LICENSE W/O VERSION CONVERSION FROM 512 TO 2048 POWER TAGS, SINGLE LICENSE",838,"TEM",1,"Simatic",0.14899999999999999,0]
["6AV63712BP074AX0","WINCC POWERPACK RT 65536/102400 FOR SIMATIC WINCC V7.4, RT LICENSE W/O VERSION CONVERSION FROM 65536 TO 102400 POWER TAGS, SINGLE LICENSE, LICENSE KEY ON USB STICK",2699,"TEM",1,"Simatic",0.14799999999999999,0]
["6AV63712BR173AJ0","WINCC POWERP. RC 153600/262144 FOR SIMATIC WINCC V7.3, RT + CS LICENSE W/O VERSION CONVERSION FROM 153600 TO 262144 POWER TAGS, FLOATING LICENSE SW AND LICENSE KEY DOWNLOAD ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY!",4162,"TEM",1,"Simatic",1E-3,0]
["6AV63722DG073AA0","WINCC/PERFORMANCE MON. BASIC P, INCL. 30 ARCHIVE-TAGS, FOR SIMATIC WINCC V7.3, RUNTIME SW ON CD, SINGLE LICENSE, LICENSE KEY ON USB-STICK",2702,"TEM",1,"Simatic",0.23100000000000001,0]
["6AV63811KA000AX5","WINCC SOFTWARE UPDATE SERVICE DOWNLOAD VALID FOR 1 LICENSE AUTOMATIC UPDATE  WITH UPGRADES AND SERVICE PACKS WITHIN THE FRAMEWORK OF THIS CONTRACT, YOU WILL RECEIVE UPDATED SOFTWARE VERSIONS FOR A PERIOD OF ONE YEAR. EXTENDED BY ANOTHER YEAR, IF IT IS NOT CANCELED THREE MONTHS PRIOR TO ITS EXPIRATION. PERIOD OF DELIVERY AND PERFORMANCE: 1 YEAR FROM DATE OF INVOICE PREREQUISITE FOR CONTRACT: CURRENT VERSION OF THE SOFTWARE ****************************** E-MAIL ADDRESS IS MANDATORY FOR DELIVERY",996,"TEM",1,"Simatic",1E-3,0]
["6AV63812BC074AH0","WINCC SYSTEMSOFTWARE V7.4, RT 128 (128 POWER TAGS), RUNTIME-SW, SINGLE LICENSE, SW AND LICENSE KEY DOWNLOAD CLASS A, 5-LANGUAGES (DE,EN,IT,FR,SP), EXECUTABLE UNDER WINDOWS 7 PROF/ENT/ULT +SP1 (32 BIT)/ 7 PROF/ENT/ULT +SP1 (64 BIT)/ 8.1 PROF/ENT (32 BIT)/ 8.1 PROF/ENT (64 BIT)/ 10 PROF/ENT (64 BIT)/ SERVER2008 R2 +SP1 (64 BIT)/ SERVER 2012 R2 (64 BIT) ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY!",2379,"TEM",1,"Simatic",1E-3,0]
["6AV63812BH074AX0","WINCC SYSTEMSOFTWARE V7.4, RT 8192 (8192 POWER TAGS), RUNTIME-SW, SINGLE LICENSE, SW AND DOCUMENTATION ON DVD, LICENSE KEY ON USB STICK, CLASS A, 5-LANGUAGES (DE,EN,IT,FR,SP), EXECUTABLE UNDER WINDOWS 7 PROF/ENT/ULT +SP1 (32 BIT)/ 7 PROF/ENT/ULT +SP1 (64 BIT)/ 8.1 PROF/ENT (32 BIT)/ 8.1 PROF/ENT (64 BIT)/ 10 PROF/ENT (64 BIT)/ SERVER2008 R2 +SP1 (64 BIT)/ SERVER 2012 R2 (64 BIT)",5397,"TEM",1,"Simatic",0.32700000000000001,0]
["6AV63812BN072AH0","WINCC SYSTEMSOFTWARE V7.2, RC 512 (512 POWER TAGS), RUNTIME & CONFIGURATION -SW FLOATING LICENSE, SW AND LICENSE KEY DOWNLOAD CLASS A, 5-LANGUAGES (DE,EN,IT,FR,SP), EXECUTABLE UNDER WINDOWS XP PROF +SP3 (32 BIT), 7 PROF/ENT/ULT +SP1 (32 BIT), 7 PROF/ENT/ULT +SP1 (64 BIT), SERVER2003 +SP2 (32 BIT), SERVER2003 R2 +SP2 (32 BIT), SERVER2008 +SP2 (32 BIT), SERVER2008 R2 +SP1 (64 BIT) ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY!",6255,"TEM",1,"Simatic",1E-3,0]
["6AV63812BU072AX0","WINCC SYSTEMSOFTWARE V7.2, RC 153600 (153600 POWER TAGS), RUNTIME & CONFIGURATION -SW ON DVD, FLOATING LICENSE, LICENSE KEY ON USB STICK, CLASS A, 5-LANGUAGES (DE,EN,IT,FR,SP), EXECUTABLE UNDER WINDOWS XP PROF +SP3 (32 BIT), 7 PROF/ENT/ULT +SP1 (32 BIT), 7 PROF/ENT/ULT +SP1 (64 BIT), SERVER2003 +SP2 (32 BIT), SERVER2003 R2 +SP2 (32 BIT), SERVER2008 +SP2 (32 BIT), SERVER2008 R2 +SP1 (64 BIT)",13320,"TEM",1,"Simatic",0.1,0]
["6AV63822HA073AX0","WINCC PACKAGE FOR SIMATIC IPC, CONSISTING OF: WINCC RT 8192, V7.3, CONNECTION VIA ON-BOARD INTERFACES, AVAILABLE ONLY W. SAME QTY OF SIMATIC IPC ON SAME ORDER FORM",4334,"TEM",1,"Simatic",0.1,0]
["6AV96811JH072DG0","WINCC/WEB NAVIGATOR V7.2, POWERPACK FROM 50 TO 100 CLIENTS, RUNTIME-SW, SINGLE LICENSE, LICENSE KEY DOWNLOAD ******************************* E-MAIL ADDRESS IS MANDATORY FOR DELIVERY!",15640,"TEM",1,"Simatic",1.4999999999999999E-2,0]
["1LE10011BA222AA4","SIMOTICS GP MOTOR TYPE: 1AV2112A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 2POLE * FS112M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, without motor protection TERMINAL BOX AT TOP",447,"TEM",1,"LD",27,1]
["1LE15012AA522AA4","SIMOTICS SD MOTOR TYPE: 1CV2205A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS200L * 37KW (50HZ) 41.5KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, without motor protection TERMINAL BOX AT TOP",3037,"TEM",1,"LD",225,1]
["1LE10010DB234AA4","SIMOTICS GP MOTOR TYPE: 1AV2082B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY 4POLE * FS80M * 0.55KW (50HZ) 60HZ: IEC 60034-30 0.63KW, 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, without motor protection TERMINAL BOX AT TOP",184,"TEM",1,"LD",10,1]
["1LE10011CB222AA4","SIMOTICS GP MOTOR TYPE: 1AV2132B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS132M * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, without motor protection TERMINAL BOX AT TOP",768,"TEM",1,"LD",49,1]
["1LE15012CB222AA4","SIMOTICS SD MOTOR TYPE: 1CV2252B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS250M * 55KW (50HZ) 63KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, without motor protection TERMINAL BOX AT TOP",4142,"TEM",1,"LD",385,1]
["1LE10011BC222AA4","SIMOTICS GP MOTOR TYPE: 1AV2112C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 6POLE * FS112M * 2.2KW (50HZ) 2.55KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, without motor protection TERMINAL BOX AT TOP",431,"TEM",1,"LD",29,1]
["1LE15012AC534AA4","SIMOTICS SD MOTOR TYPE: 1CV2205C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS200L * 22KW (50HZ) 26.5KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, without motor protection TERMINAL BOX AT TOP",2782,"TEM",1,"LD",220,1]
["1LE10010DA334FB4","SIMOTICS GP MOTOR TYPE: 1AV2083A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 2POLE * FS80M * 1.1KW (50HZ) 1.27KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF165(A200) 1 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP",247,"TEM",1,"LD",11,1]
["1LE15012BA234FB4","SIMOTICS SD MOTOR TYPE: 1CV2222A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS225M * 45KW (50HZ) 51KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF400(A450) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP",3915,"TEM",1,"LD",0.29499999999999998,1]
["1LE15012DA234FB4","SIMOTICS SD MOTOR TYPE: 1CV2282A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS280M * 90KW (50HZ) 101KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF500(A550) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP",7426,"TEM",1,"LD",530,1]
["1LE10011CB034FA4","SIMOTICS GP MOTOR TYPE: 1AV2130B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! (01.01.2017) 4POLE * FS132S * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF265(A300) without motor protection TERMINAL BOX AT TOP",656,"TEM",1,"LD",4.2000000000000003E-2,1]
["1LE15012BB234FA4","SIMOTICS SD MOTOR TYPE: 1CV2222B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS225M * 45KW (50HZ) 52KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF400(A450) without motor protection TERMINAL BOX AT TOP TERMINAL BOX AT TOP",3574,"TEM",1,"LD",0.30499999999999999,1]
["1LE15012BC222FB4","SIMOTICS SD MOTOR TYPE: 1CV2222C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS225M * 30KW (50HZ) 36KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 5, FLANGE: FF400(A450) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP",4017,"TEM",1,"LD",300,1]
["1LE15012BC222FA4","SIMOTICS SD MOTOR TYPE: 1CV2222C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS225M * 30KW (50HZ) 36KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 5, FLANGE: FF400(A450) without motor protection TERMINAL BOX AT TOP",3891,"TEM",1,"LD",300,1]
["1LE10011DA434GB4","SIMOTICS GP MOTOR TYPE: 1AV2164A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS160L * 18.5KW (50HZ) 21.3KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP",1674,"TEM",1,"LD",84,1]
["1LE15013AA222GA4","SIMOTICS SD MOTOR TYPE: 1CV2312A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 2POLE * FS315M * 132KW (50HZ) 148KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, FLANGE: FF600(A660) without motor protection TERMINAL BOX AT TOP",10439,"TEM",1,"LD",880,1]
["1LE10011DB434WB4","SIMOTICS GP MOTOR TYPE: 1AV2164B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING HIGH EFFICIENCY IE2, IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION! 4POLE * FS160L * 15KW (50HZ) 17.3KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 15 * FLANGE: FF300 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP",1470,"TEM",1,"LD",83,1]
["1LE15013AC434GB4","SIMOTICS SD MOTOR TYPE: 1CV2314C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE HIGH EFFICIENCY IE2, 60HZ, P60: IE1 IN EEA: CONSIDER EFFIC. GRADE ACC. TO CURR. VALID REGULATION 6POLE * FS315L * 110KW (50HZ) 132KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP",12625,"TEM",1,"LD",940,1]
["1LE10030EA422AB4","SIMOTICS GP MOTOR TYPE: 1AV3094A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS90L * 2.2KW (50HZ) 2.55KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 1 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP",394,"TEM",1,"LD",19.001000000000001,1]
["1LE15032DA034AB4","SIMOTICS SD MOTOR TYPE: 1CV3280A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 2POLE * FS280S * 75KW (50HZ) 84KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP",6450,"TEM",1,"LD",510,1]
["1LE10030EB034AA4","SIMOTICS GP MOTOR TYPE: 1AV3090B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 4POLE * FS90S * 1.1KW (50HZ) 1.27KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, without motor protection TERMINAL BOX AT TOP",285,"TEM",1,"LD",16,1]
["1LE15031EB434AA4","SIMOTICS SD MOTOR TYPE: 1CV3184B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 4POLE * FS180L * 22KW (50HZ) 25.3KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, without motor protection TERMINAL BOX AT TOP",2030,"TEM",1,"LD",170,1]
["1LE15033AB234AA4","SIMOTICS SD MOTOR TYPE: 1CV3312B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 4POLE * FS315M * 132KW (50HZ) 152KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, without motor protection TERMINAL BOX AT TOP",10313,"TEM",1,"LD",960,1]
["1LE10031DC222AB4","SIMOTICS GP MOTOR TYPE: 1AV3162C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS160M * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B3 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP",1268,"TEM",1,"LD",93,1]
["1LE15032DC222AB4","SIMOTICS SD MOTOR TYPE: 1CV3282C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS280M * 55KW (50HZ) 66KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP",7140,"TEM",1,"LD",560,1]
["1LE10030EA434FB4","SIMOTICS GP MOTOR TYPE: 1AV3094A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 2POLE * FS90L * 2.2KW (50HZ) 2.55KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF165(A200) 1 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP",420,"TEM",1,"LD",19.001000000000001,1]
["1LE15032AA534FB4","SIMOTICS SD MOTOR TYPE: 1CV3205A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS200L * 37KW (50HZ) 41.5KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF350(A400) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP",3572,"TEM",1,"LD",250,1]
["1LE10030DB334FA4","SIMOTICS GP MOTOR TYPE: 1AV3083B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 4POLE * FS80M * 0.75KW (50HZ) 0.86KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF165(A200) without motor protection TERMINAL BOX AT TOP",262,"TEM",1,"LD",14,1]
["1LE15032BB034FB4","SIMOTICS SD MOTOR TYPE: 1CV3220B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 4POLE * FS225S * 37KW (50HZ) 42.5KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF400(A450) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP",3412,"TEM",1,"LD",285,1]
["1LE15033AB022FA4","SIMOTICS SD MOTOR TYPE: 1CV3310B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 4POLE * FS315S * 110KW (50HZ) 127KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 5, FLANGE: FF600(A660) without motor protection TERMINAL BOX AT TOP",9095,"TEM",1,"LD",760,1]
["1LE15033AC034FB4","SIMOTICS SD MOTOR TYPE: 1CV3310C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 6POLE * FS315S * 75KW (50HZ) 90KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 5, FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP",10064,"TEM",1,"LD",750,1]
["1LE10031BA222GA4","SIMOTICS GP MOTOR TYPE: 1AV3112A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 2POLE * FS112M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, without motor protection TERMINAL BOX AT TOP",543,"TEM",1,"LD",34,1]
["1LE15032AA522GA4","SIMOTICS SD MOTOR TYPE: 1CV3205A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS200L * 37KW (50HZ) 41.5KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, FLANGE: FF350(A400) without motor protection TERMINAL BOX AT TOP",3480,"TEM",1,"LD",250,1]
["1LE15033AA522GA4","SIMOTICS SD MOTOR TYPE: 1CV3315A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE PREMIUM EFFICIENCY IE3, 2POLE * FS315L * 200KW (50HZ) 224KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, FLANGE: FF600(A660) without motor protection TERMINAL BOX AT TOP",17146,"TEM",1,"LD",1150,1]
["1LE10031CC234WB4","SIMOTICS GP MOTOR TYPE: 1AV3132C LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE3, 60HZ, P60: IE2 6POLE * FS132M * 4KW (50HZ) 4.55KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 15 * FLANGE: FF265 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP",885,"TEM",1,"LD",52,1]
["1LE10041DA222AA4","SIMOTICS GP MOTOR TYPE: 1AV4162A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 2POLE * FS160M * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, without motor protection TERMINAL BOX AT TOP",1348,"TEM",1,"LD",84,1]
["1LE15042DA234AB4","SIMOTICS SD MOTOR TYPE: 1CV4282A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 2POLE * FS280M * 90KW (50HZ) 101KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM B 3, 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP",8683,"TEM",1,"LD",610,1]
["1LE10041CB022AA4","SIMOTICS GP MOTOR TYPE: 1AV4130B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 4POLE * FS132S * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, without motor protection TERMINAL BOX AT TOP",829,"TEM",1,"LD",59,1]
["1LE15042DB022AA4","SIMOTICS SD MOTOR TYPE: 1CV4280B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 4POLE * FS280S * 75KW (50HZ) 86KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 3, without motor protection TERMINAL BOX AT TOP",6862,"TEM",1,"LD",670,1]
["1LE10041CA022FB4","SIMOTICS GP MOTOR TYPE: 1AV4130A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 2POLE * FS132S * 5.5KW (50HZ) 6.3KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 5, FLANGE: FF265(A300) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP",884,"TEM",1,"LD",44,1]
["1LE15042BA222FB4","SIMOTICS SD MOTOR TYPE: 1CV4222A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 2POLE * FS225M * 45KW (50HZ) 51KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 5, FLANGE: FF400(A450) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP",4837,"TEM",1,"LD",330,1]
["1LE10041CB222FA4","SIMOTICS GP MOTOR TYPE: 1AV4132B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 4POLE * FS132M * 7.5KW (50HZ) 8.6KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 5, FLANGE: FF265(A300) without motor protection TERMINAL BOX AT TOP",1099,"TEM",1,"LD",62,1]
["1LE15042CB222FA4","SIMOTICS SD MOTOR TYPE: 1CV4252B LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 4POLE * FS250M * 55KW (50HZ) 63KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM B 5, FLANGE: FF500(A550) without motor protection TERMINAL BOX AT TOP",5312,"TEM",1,"LD",490,1]
["1LE10041DA222GB4","SIMOTICS GP MOTOR TYPE: 1AV4162A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) ALUMINIUM HOUSING PREMIUM EFFICIENCY IE4, 2POLE * FS160M * 11KW (50HZ) 12.6KW (60HZ) 3 AC 50HZ 230VD/400VY * 3 AC 60HZ 460VY IM V 1 W/O CANOPY, FLANGE: FF300(A350) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP",1484,"TEM",1,"LD",84,1]
["1LE15043AA034GB4","SIMOTICS SD MOTOR TYPE: 1CV4310A LOW-VOLTAGE MOTOR, IEC SQUIRREL-CAGE,SELF-VENTIL.,IP55 TEMP. CL. 155(F) ACC.TO 130(B) CAST-IRON HOUSING BASIC LINE SUPER PREMIUM EFFICIENCY IE4, 2POLE * FS315S * 110KW (50HZ) 123KW (60HZ) 3 AC 50HZ 400VD/690VY * 3 AC 60HZ 460VD IM V 1 W/O CANOPY, FLANGE: FF600(A660) 3 PTC thermistor for tripping (2 terminals) TERMINAL BOX AT TOP",10677,"TEM",1,"LD",750,1]
["1FK70115AK711JH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.18NM, 100K, 6000RPM, 0,05KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1312,"TEM",1,"MC",1.101,1]
["1FK70155AK711JH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.35 NM, 100 K, 6000 RPM,0,10KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. DEGREE OF PROTECTION IP54; PAINT FINISH RAL7016 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE",1396,"TEM",1,"MC",1.3009999999999999,1]
["1FK70225AK211AB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1842,"TEM",1,"MC",2.0019999999999998,1]
["1FK70225AK211HH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2406,"TEM",1,"MC",2.0019999999999998,1]
["1FK70225AK211LH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2552,"TEM",1,"MC",2.0019999999999998,1]
["1FK70225AK211SG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",923,"TEM",1,"MC",1.8029999999999999,1]
["1FK70225AK211UA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 0.85 NM, 100 K, 6000 RPM, 0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER MULTI-POLE (RESOLVER P=3); WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1284,"TEM",1,"MC",1.8029999999999999,1]
["1FK70225AK711AA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1710,"TEM",1,"MC",1.8029999999999999,1]
["1FK70225AK711DG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1937,"TEM",1,"MC",1.8029999999999999,1]
["1FK70225AK711JB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1705,"TEM",1,"MC",2.0019999999999998,1]
["1FK70225AK711PA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1517,"TEM",1,"MC",1.8029999999999999,1]
["1FK70225AK711SH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1249,"TEM",1,"MC",2.0019999999999998,1]
["1FK70225AK711VA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 0.85 NM, 100K, 6000 RPM,0,38KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1977,"TEM",1,"MC",1.8029999999999999,1]
["1FK70225AK717SH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 0.85 NM ,100 K, 6000 RPM, 0,38KW NATURAL COOLING, FREE CABLE END 0.5 M, OUTGOING CONNECTOR DIRECTION NON-DRIVE END WITH CONNECTOR SIZE 1 FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1368,"TEM",1,"MC",2.0019999999999998,1]
["1FK70322AF211BH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1964,"TEM",1,"MC",3,1]
["1FK70322AF211PG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,31 KW; UZK=300V M0=1,2NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1255,"TEM",1,"MC",2.8010000000000002,1]
["1FK70322AK711AB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1905,"TEM",1,"MC",3,1]
["1FK70322AK711AG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1506,"TEM",1,"MC",2.7010000000000001,1]
["1FK70322AK711QB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1663,"TEM",1,"MC",3,1]
["1FK70322AK711TA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,5 KW; UZK=600V M0=1,15NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1100,"TEM",1,"MC",2.702,1]
["1FK70325AF211AH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1973,"TEM",1,"MC",3.0019999999999998,1]
["1FK70325AF211HB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2522,"TEM",1,"MC",3.0019999999999998,1]
["1FK70325AF211LB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2679,"TEM",1,"MC",3.0019999999999998,1]
["1FK70325AF211PH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1647,"TEM",1,"MC",3.0019999999999998,1]
["1FK70325AF211TG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1000,"TEM",1,"MC",2.7029999999999998,1]
["1FK70325AF211VB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, ZK 300 V 1.1 NM, 100 K, 3000 RPM, 0.31KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2328,"TEM",1,"MC",3.0019999999999998,1]
["1FK70325AK711DA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2093,"TEM",1,"MC",2.7029999999999998,1]
["1FK70325AK711HG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2190,"TEM",1,"MC",2.7029999999999998,1]
["1FK70325AK711LG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2400,"TEM",1,"MC",2.7029999999999998,1]
["1FK70325AK711SA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1244,"TEM",1,"MC",2.7029999999999998,1]
["1FK70325AK711TH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1235,"TEM",1,"MC",3.0019999999999998,1]
["1FK70325AK711VG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 COMPACT, 1.1 NM, 100 K, 6000 RPM, 0.50KW, NATURAL COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1996,"TEM",1,"MC",2.7029999999999998,1]
["1FK70334CF211BH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2102,"TEM",1,"MC",3.3,1]
["1FK70334CF211SH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,38 KW; UZK=300V M0=1,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1181,"TEM",1,"MC",3.3010000000000002,1]
["1FK70334CK711AB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1949,"TEM",1,"MC",3.3,1]
["1FK70334CK711DG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1872,"TEM",1,"MC",3.0019999999999998,1]
["1FK70334CK711RA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1863,"TEM",1,"MC",3.0009999999999999,1]
["1FK70334CK711TH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,57 KW; UZK=600V M0=1,3NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1275,"TEM",1,"MC",3.3010000000000002,1]
["1FK70337AF211DB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2277,"TEM",1,"MC",3.4020000000000001,1]
["1FK70337AF211HH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2372,"TEM",1,"MC",3.4020000000000001,1]
["1FK70337AF211LB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 512 P/REV (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2938,"TEM",1,"MC",3.4020000000000001,1]
["1FK70337AF211SB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1530,"TEM",1,"MC",3.4020000000000001,1]
["1FK70337AF211TH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1434,"TEM",1,"MC",3.4020000000000001,1]
["1FK70337AF211VG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 1.3 NM, 100 K, 3000 RPM, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1887,"TEM",1,"MC",3.1030000000000002,1]
["1FK70337AK711DG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1946,"TEM",1,"MC",3.1030000000000002,1]
["1FK70337AK711JA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 16 S/R (ENCODER A-16); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1668,"TEM",1,"MC",3.1030000000000002,1]
["1FK70337AK711PA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1505,"TEM",1,"MC",3.1030000000000002,1]
["1FK70337AK711SG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 1.3 NM, 100 K, 6000 RPM, 0.57KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1198,"TEM",1,"MC",3.1030000000000002,1]
["1FK70342AF211AA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1688,"TEM",1,"MC",3.7010000000000001,1]
["1FK70342AF211DG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1923,"TEM",1,"MC",3.702,1]
["1FK70342AF211QA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1539,"TEM",1,"MC",3.7010000000000001,1]
["1FK70342AF211TG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,47 KW; UZK=300V M0=1,6NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1109,"TEM",1,"MC",3.702,1]
["1FK70342AK711AH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1911,"TEM",1,"MC",4,1]
["1FK70342AK711EA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2153,"TEM",1,"MC",3.7010000000000001,1]
["1FK70342AK711QG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1453,"TEM",1,"MC",3.7010000000000001,1]
["1FK70342AK711TB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,63 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1414,"TEM",1,"MC",4.0010000000000003,1]
["1FK70345AF211AG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, ZK 300 V 1.6 NM, 100 K, 3000 RPM 0.46KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEG. INCREMENTAL ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1788,"TEM",1,"MC",3.7029999999999998,1]
["1FK70345AF211HG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, ZK 300 V 1.6 NM, 100 K, 3000 RPM 0.46KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEG. ABSOLUTE ENCODER 512 S/R (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2244,"TEM",1,"MC",3.7029999999999998,1]
["1FK70345AF211LA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, ZK 300 V 1.6 NM, 100 K, 3000 RPM 0.46KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEG. ABSOLUTE ENCODER 512 S/R (ENCODER A-512) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2647,"TEM",1,"MC",3.7029999999999998,1]
["1FK70345AF211SA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, ZK 300 V 1.6 NM, 100 K, 3000 RPM 0.46KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEG. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1246,"TEM",1,"MC",3.7029999999999998,1]
["1FK70345AF211TG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, ZK 300 V 1.6 NM, 100 K, 3000 RPM 0.46KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEG. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1362,"TEM",1,"MC",3.7029999999999998,1]
["1FK70345AF211VB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, ZK 300 V 1.6 NM, 100 K, 3000 RPM 0.46KW, NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEG. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2322,"TEM",1,"MC",4.0019999999999998,1]
["1FK70345AK711DA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 1.6 NM, 100 K, 6000 RPM, 0,63KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEG. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2354,"TEM",1,"MC",3.7029999999999998,1]
["1FK70345AK711HH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 1.6 NM, 100 K, 6000 RPM, 0,63KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEG. ABSOLUTE ENCODER 512 S/R (ENCODER A-512); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2378,"TEM",1,"MC",4.0019999999999998,1]
["1FK70345AK711SA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 1.6 NM, 100 K, 6000 RPM, 0,63KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEG. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1456,"TEM",1,"MC",3.7029999999999998,1]
["1FK70345AK711UA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 1.6 NM, 100 K, 6000 RPM, 0,63KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEG. RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1609,"TEM",1,"MC",3.7029999999999998,1]
["1FK70345AK711VH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 COMPACT, 1.6 NM, 100 K, 6000 RPM, 0,63KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEG. BASIC ABSOLUTE ENCODER 16 P/REV (ENCODER A-16) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2075,"TEM",1,"MC",4.0019999999999998,1]
["1FK70402AK711CH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,69 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2440,"TEM",1,"MC",3.5,1]
["1FK70402AK711PH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,69 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1484,"TEM",1,"MC",3.6,1]
["1FK70402AK711SB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,69 KW; UZK=600V M0=1,6NM (100K); NN=6000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1425,"TEM",1,"MC",3.5009999999999999,1]
["1FK70405AK711AB5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 1.6 NM, 100 K, 6000 RPM 0.69KW, NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2234,"TEM",1,"MC",4.1020000000000003,1]
["1FK70405AK711DH3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 1.6 NM, 100 K, 6000 RPM 0.69KW, NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2298,"TEM",1,"MC",4.1020000000000003,1]
["1FK70405AK711FH5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 1.6 NM, 100 K, 6000 RPM 0.69KW, NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2800,"TEM",1,"MC",4.1020000000000003,1]
["1FK70405AK711KG0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 1.6 NM, 100 K, 6000 RPM 0.69KW, NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1807,"TEM",1,"MC",3.5030000000000001,1]
["1FK70405AK711SA3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 1.6 NM, 100 K, 6000 RPM 0.69KW, NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1212,"TEM",1,"MC",3.5030000000000001,1]
["1FK70405AK711UA2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 1.6 NM, 100 K, 6000 RPM 0.69KW, NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1526,"TEM",1,"MC",3.5030000000000001,1]
["1FK70422AC711BA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,59 KW; UZK=600V M0=3NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2055,"TEM",1,"MC",4.601,1]
["1FK70422AC711EA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,59 KW; UZK=600V M0=3NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2186,"TEM",1,"MC",4.601,1]
["1FK70422AC711PG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,59 KW; UZK=600V M0=3NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1383,"TEM",1,"MC",4.7009999999999996,1]
["1FK70422AF211AB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,82 KW; UZK=300V M0=3NM (100K); NN=3000RPM; NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2075,"TEM",1,"MC",4.9000000000000004,1]
["1FK70422AF211AG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,82 KW; UZK=300V M0=3NM (100K); NN=3000RPM; NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1728,"TEM",1,"MC",4.601,1]
["1FK70422AF211PB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,82 KW; UZK=300V M0=3NM (100K); NN=3000RPM; NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1637,"TEM",1,"MC",5,1]
["1FK70422AF211SG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,82 KW; UZK=300V M0=3NM (100K); NN=3000RPM; NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1049,"TEM",1,"MC",4.6020000000000003,1]
["1FK70422AF711AH0","SIMOTICS S SIMOTICS S-1FK7 SYNCHRONOUS MOTOR 1FK7-CT PN=0,82 KW; UZK=600V M0=3NM (100K); NN=3000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1893,"TEM",1,"MC",4.9000000000000004,1]
["1FK70422AF711DG0","SIMOTICS S SIMOTICS S-1FK7 SYNCHRONOUS MOTOR 1FK7-CT PN=0,82 KW; UZK=600V M0=3NM (100K); NN=3000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1956,"TEM",1,"MC",4.6020000000000003,1]
["1FK70422AF711KG1","SIMOTICS S SIMOTICS S-1FK7 SYNCHRONOUS MOTOR 1FK7-CT PN=0,82 KW; UZK=600V M0=3NM (100K); NN=3000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 16BIT + 12BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM16DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1901,"TEM",1,"MC",4.601,1]
["1FK70422AF711RB0","SIMOTICS S SIMOTICS S-1FK7 SYNCHRONOUS MOTOR 1FK7-CT PN=0,82 KW; UZK=600V M0=3NM (100K); NN=3000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2114,"TEM",1,"MC",4.9000000000000004,1]
["1FK70422AF711TH2","SIMOTICS S SIMOTICS S-1FK7 SYNCHRONOUS MOTOR 1FK7-CT PN=0,82 KW; UZK=600V M0=3NM (100K); NN=3000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1401,"TEM",1,"MC",4.9009999999999998,1]
["1FK70422AK711CA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,94 KW; UZK=600V M0=3NM (100K); NN=6000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2331,"TEM",1,"MC",4.601,1]
["1FK70422AK711FG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,94 KW; UZK=600V M0=3NM (100K); NN=6000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2325,"TEM",1,"MC",4.601,1]
["1FK70422AK711RA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=0,94 KW; UZK=600V M0=3NM (100K); NN=6000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1947,"TEM",1,"MC",4.601,1]
["1FK70423BK711BB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI; PN=0,94 KW; UZK=600V M0=3NM (100K); NN=6000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2223,"TEM",1,"MC",5.4,1]
["1FK70423BK711BH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI; PN=0,94 KW; UZK=600V M0=3NM (100K); NN=6000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2228,"TEM",1,"MC",5.4,1]
["1FK70423BK711QA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI; PN=0,94 KW; UZK=600V M0=3NM (100K); NN=6000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1572,"TEM",1,"MC",5.101,1]
["1FK70425AC711DB3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 3.0 NM, 100 K, 2000 RPM, 0,59KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2463,"TEM",1,"MC",5.5019999999999998,1]
["1FK70425AF211AA8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, ZK 300 V 3,0 NM, 100K, 3000 RPM, 0,82KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2128,"TEM",1,"MC",4.9029999999999996,1]
["1FK70425AF211AB2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, ZK 300 V 3,0 NM, 100K, 3000 RPM, 0,82KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2254,"TEM",1,"MC",5.5019999999999998,1]
["1FK70425AF211FH0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, ZK 300 V 3,0 NM, 100K, 3000 RPM, 0,82KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2719,"TEM",1,"MC",5.5019999999999998,1]
["1FK70425AF211KB3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, ZK 300 V 3,0 NM, 100K, 3000 RPM, 0,82KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2302,"TEM",1,"MC",5.5019999999999998,1]
["1FK70425AF211SB2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, ZK 300 V 3,0 NM, 100K, 3000 RPM, 0,82KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1618,"TEM",1,"MC",5.5019999999999998,1]
["1FK70425AF211TG8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, ZK 300 V 3,0 NM, 100K, 3000 RPM, 0,82KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1398,"TEM",1,"MC",4.9029999999999996,1]
["1FK70425AF711AH2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 3.0 NM, 100K, 3000 RPM, 0,82KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2158,"TEM",1,"MC",5.5019999999999998,1]
["1FK70425AF711EB5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 3.0 NM, 100K, 3000 RPM, 0,82KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10%  DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2707,"TEM",1,"MC",5.5019999999999998,1]
["1FK70425AF711FH8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 3.0 NM, 100K, 3000 RPM, 0,82KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2979,"TEM",1,"MC",5.5019999999999998,1]
["1FK70425AF711KH3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 3.0 NM, 100K, 3000 RPM, 0,82KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2206,"TEM",1,"MC",5.5019999999999998,1]
["1FK70425AF711SB8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 3.0 NM, 100K, 3000 RPM, 0,82KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1775,"TEM",1,"MC",5.5019999999999998,1]
["1FK70425AF711UB5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 3.0 NM, 100K, 3000 RPM, 0,82KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1929,"TEM",1,"MC",5.5019999999999998,1]
["1FK70425AK711AH8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 3.0 NM, 100 K, 6000 RPM,1.02KW, NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2316,"TEM",1,"MC",5.5019999999999998,1]
["1FK70425AK711EG2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 3.0 NM, 100 K, 6000 RPM,1.02KW, NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10%  DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2280,"TEM",1,"MC",4.9029999999999996,1]
["1FK70425AK711GG0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 3.0 NM, 100 K, 6000 RPM,1.02KW, NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1617,"TEM",1,"MC",4.9029999999999996,1]
["1FK70425AK711SG0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 3.0 NM, 100 K, 6000 RPM,1.02KW, NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1139,"TEM",1,"MC",4.9029999999999996,1]
["1FK70425AK711UG0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 3.0 NM, 100 K, 6000 RPM,1.02KW, NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1401,"TEM",1,"MC",4.9029999999999996,1]
["1FK70434CF211CB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,94 KW; UZK=300V M0=3,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2730,"TEM",1,"MC",6.3,1]
["1FK70434CF211PA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,94 KW; UZK=300V M0=3,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1420,"TEM",1,"MC",6.101,1]
["1FK70434CF211SB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,94 KW; UZK=300V M0=3,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1440,"TEM",1,"MC",6.3010000000000002,1]
["1FK70434CF211UH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=0,94 KW; UZK=300V M0=3,3NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1686,"TEM",1,"MC",6.3010000000000002,1]
["1FK70434CH711CG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,2 KW; UZK=600V M0=3,5NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2383,"TEM",1,"MC",6.0010000000000003,1]
["1FK70434CH711PG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,2 KW; UZK=600V M0=3,5NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1427,"TEM",1,"MC",6.101,1]
["1FK70434CH711SB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,2 KW; UZK=600V M0=3,5NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1534,"TEM",1,"MC",6.3010000000000002,1]
["1FK70434CK711AA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,3 KW; UZK=600V M0=3,5NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1765,"TEM",1,"MC",6.0010000000000003,1]
["1FK70434CK711CA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,3 KW; UZK=600V M0=3,5NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2469,"TEM",1,"MC",6.0010000000000003,1]
["1FK70434CK711PH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,3 KW; UZK=600V M0=3,5NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1593,"TEM",1,"MC",6.4,1]
["1FK70434CK711TA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,3 KW; UZK=600V M0=3,5NM (100K); NN=6000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1179,"TEM",1,"MC",6.0019999999999998,1]
["1FK70437AF211AB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 3.1 NM, 100 K, 3000 RPM, 0.79KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2351,"TEM",1,"MC",6.9020000000000001,1]
["1FK70437AF211EA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 3.1 NM, 100 K, 3000 RPM, 0.79KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10%  DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2320,"TEM",1,"MC",6.3029999999999999,1]
["1FK70437AF211FH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 3.1 NM, 100 K, 3000 RPM, 0.79KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3027,"TEM",1,"MC",6.9020000000000001,1]
["1FK70437AF211KG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 3.1 NM, 100 K, 3000 RPM, 0.79KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2026,"TEM",1,"MC",6.3029999999999999,1]
["1FK70437AF211SG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, ZK 300 V 3.1 NM, 100 K, 3000 RPM, 0.79KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1187,"TEM",1,"MC",6.3029999999999999,1]
["1FK70437AH711AH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 3.1 NM, 100 K, 4500 RPM, 1,23KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2364,"TEM",1,"MC",6.9020000000000001,1]
["1FK70437AH711EG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 3.1 NM, 100 K, 4500 RPM, 1,23KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10%  DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2328,"TEM",1,"MC",6.3029999999999999,1]
["1FK70437AH711FG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 3.1 NM, 100 K, 4500 RPM, 1,23KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2535,"TEM",1,"MC",6.3029999999999999,1]
["1FK70437AH711PA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 3.1 NM, 100 K, 4500 RPM, 1,23KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1644,"TEM",1,"MC",6.3029999999999999,1]
["1FK70437AH711SG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 3.1 NM, 100 K, 4500 RPM, 1,23KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1338,"TEM",1,"MC",6.3029999999999999,1]
["1FK70437AH711UG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 3.1 NM, 100 K, 4500 RPM, 1,23KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1498,"TEM",1,"MC",6.3029999999999999,1]
["1FK70437AK711DA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 3.1 NM, 100 K, 6000 RPM, 1.26KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2438,"TEM",1,"MC",6.3029999999999999,1]
["1FK70437AK711FA5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 3.1 NM, 100 K, 6000 RPM, 1.26KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2731,"TEM",1,"MC",6.3029999999999999,1]
["1FK70437AK711GH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 3.1 NM, 100 K, 6000 RPM, 1.26KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1946,"TEM",1,"MC",6.9020000000000001,1]
["1FK70437AK711PB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 3.1 NM, 100 K, 6000 RPM, 1.26KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1875,"TEM",1,"MC",6.9020000000000001,1]
["1FK70437AK711TB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 3.1 NM, 100 K, 6000 RPM, 1.26KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1666,"TEM",1,"MC",6.9020000000000001,1]
["1FK70437AK711UH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 3.1 NM, 100 K, 6000 RPM, 1.26KW, NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1880,"TEM",1,"MC",6.9020000000000001,1]
["1FK70444CF711EH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,2 KW; UZK=600V M0=4,5NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2473,"TEM",1,"MC",7.7,1]
["1FK70444CF711KH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,2 KW; UZK=600V M0=4,5NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 16BIT + 12BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM16DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2181,"TEM",1,"MC",7.7,1]
["1FK70444CF711RB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,2 KW; UZK=600V M0=4,5NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2322,"TEM",1,"MC",7.7,1]
["1FK70444CF711UG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,2 KW; UZK=600V M0=4,5NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1498,"TEM",1,"MC",7.4020000000000001,1]
["1FK70444CH711PB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,4 KW; UZK=600V M0=4,5NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1752,"TEM",1,"MC",7.8,1]
["1FK70444CH711RH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,4 KW; UZK=600V M0=4,5NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2234,"TEM",1,"MC",7.7,1]
["1FK70447AF711AA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 4.0 NM, 100 K, 3000 RPM, 1,1KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2043,"TEM",1,"MC",7.7030000000000003,1]
["1FK70447AF711DG8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 4.0 NM, 100 K, 3000 RPM, 1,1KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2421,"TEM",1,"MC",7.7030000000000003,1]
["1FK70447AF711FG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 4.0 NM, 100 K, 3000 RPM, 1,1KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2714,"TEM",1,"MC",7.7030000000000003,1]
["1FK70447AF711GG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 4.0 NM, 100 K, 3000 RPM, 1,1KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1843,"TEM",1,"MC",7.7030000000000003,1]
["1FK70447AF711PH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 4.0 NM, 100 K, 3000 RPM, 1,1KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1908,"TEM",1,"MC",8.3019999999999996,1]
["1FK70447AF711TH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 4.0 NM, 100 K, 3000 RPM, 1,1KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1545,"TEM",1,"MC",8.3019999999999996,1]
["1FK70447AH711AB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 4.0 NM, 100 K, 4500 RPM, 1,41KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2326,"TEM",1,"MC",8.3019999999999996,1]
["1FK70447AH711DH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 4.0 NM, 100 K, 4500 RPM, 1,41KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2702,"TEM",1,"MC",8.3019999999999996,1]
["1FK70447AH711FH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 4.0 NM, 100 K, 4500 RPM, 1,41KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2995,"TEM",1,"MC",8.3019999999999996,1]
["1FK70447AH711KG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 4.0 NM, 100 K, 4500 RPM, 1,41KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2001,"TEM",1,"MC",7.7030000000000003,1]
["1FK70447AH711SB8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 4.0 NM, 100 K, 4500 RPM, 1,41KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",1900,"TEM",1,"MC",8.3019999999999996,1]
["1FK70447AH711UA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 4.0 NM, 100 K, 4500 RPM, 1,41KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1721,"TEM",1,"MC",7.7030000000000003,1]
["1FK70602AC711EB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,1 KW; UZK=600V M0=6NM (100K); NN=2000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2703,"TEM",1,"MC",7.4,1]
["1FK70602AC711KG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,1 KW; UZK=600V M0=6NM (100K); NN=2000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 16BIT + 12BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM16DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2116,"TEM",1,"MC",7.101,1]
["1FK70602AC711SH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,1 KW; UZK=600V M0=6NM (100K); NN=2000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1568,"TEM",1,"MC",7.4009999999999998,1]
["1FK70602AF711BA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,5 KW; UZK=600V M0=6NM (100K); NN=3000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2176,"TEM",1,"MC",7.101,1]
["1FK70602AF711EA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,5 KW; UZK=600V M0=6NM (100K); NN=3000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2307,"TEM",1,"MC",7.101,1]
["1FK70602AF711KB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,5 KW; UZK=600V M0=6NM (100K); NN=3000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 16BIT + 12BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM16DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2505,"TEM",1,"MC",7.4,1]
["1FK70602AF711RG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,5 KW; UZK=600V M0=6NM (100K); NN=3000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2075,"TEM",1,"MC",7.101,1]
["1FK70602AF711UB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,5 KW; UZK=600V M0=6NM (100K); NN=3000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1987,"TEM",1,"MC",7.4009999999999998,1]
["1FK70602AH711BH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,7 KW; UZK=600V M0=6NM (100K); NN=4500RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2489,"TEM",1,"MC",7.4,1]
["1FK70602AH711PG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,7 KW; UZK=600V M0=6NM (100K); NN=4500RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1598,"TEM",1,"MC",7.2009999999999996,1]
["1FK70602AH711SB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,7 KW; UZK=600V M0=6NM (100K); NN=4500RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1652,"TEM",1,"MC",7.4009999999999998,1]
["1FK70603BF711BG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI; PN=1,5 KW; UZK=600V M0=6NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2184,"TEM",1,"MC",7.8010000000000002,1]
["1FK70603BF711DA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI; PN=1,5 KW; UZK=600V M0=6NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2350,"TEM",1,"MC",7.8019999999999996,1]
["1FK70603BF711QG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI; PN=1,5 KW; UZK=600V M0=6NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1701,"TEM",1,"MC",7.8010000000000002,1]
["1FK70605AF711DA5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 6,0NM, 100K, 3000RPM, 1,48KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2515,"TEM",1,"MC",7.0030000000000001,1]
["1FK70605AF711EG5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 6,0NM, 100K, 3000RPM, 1,48KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10%  DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2563,"TEM",1,"MC",7.0030000000000001,1]
["1FK70605AF711GG2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 6,0NM, 100K, 3000RPM, 1,48KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1951,"TEM",1,"MC",7.0030000000000001,1]
["1FK70605AF711PA5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 6,0NM, 100K, 3000RPM, 1,48KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1878,"TEM",1,"MC",7.0030000000000001,1]
["1FK70605AF711UG3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 6,0NM, 100K, 3000RPM, 1,48KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1683,"TEM",1,"MC",7.0030000000000001,1]
["1FK70605AH711DB5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 6.0 NM, 100 K, 4500 RPM,1,74KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2844,"TEM",1,"MC",8.3019999999999996,1]
["1FK70605AH711FA0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 6.0 NM, 100 K, 4500 RPM,1,74KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2765,"TEM",1,"MC",7.0030000000000001,1]
["1FK70605AH711KA3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 6.0 NM, 100 K, 4500 RPM,1,74KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2252,"TEM",1,"MC",7.0030000000000001,1]
["1FK70605AH711PB8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 6.0 NM, 100 K, 4500 RPM,1,74KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2316,"TEM",1,"MC",8.3019999999999996,1]
["1FK70605AH711TA2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 6.0 NM, 100 K, 4500 RPM,1,74KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1567,"TEM",1,"MC",7.0030000000000001,1]
["1FK70614CF711AA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,7 KW; UZK=600V M0=6,4NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2046,"TEM",1,"MC",9.5009999999999994,1]
["1FK70614CF711CG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,7 KW; UZK=600V M0=6,4NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2663,"TEM",1,"MC",9.5009999999999994,1]
["1FK70614CF711PA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,7 KW; UZK=600V M0=6,4NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1794,"TEM",1,"MC",9.6010000000000009,1]
["1FK70614CF711SB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=1,7 KW; UZK=600V M0=6,4NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1856,"TEM",1,"MC",9.8010000000000002,1]
["1FK70614CH711AA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2 KW; UZK=600V M0=6,4NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2139,"TEM",1,"MC",9.5009999999999994,1]
["1FK70614CH711CH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2 KW; UZK=600V M0=6,4NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2875,"TEM",1,"MC",9.8000000000000007,1]
["1FK70614CH711QA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2 KW; UZK=600V M0=6,4NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1804,"TEM",1,"MC",9.5009999999999994,1]
["1FK70614CH711TB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2 KW; UZK=600V M0=6,4NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1763,"TEM",1,"MC",9.8010000000000002,1]
["1FK70617AF711AG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 6.4 NM, 100 K, 3000 RPM, 1,70KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2128,"TEM",1,"MC",10.003,1]
["1FK70617AF711FH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 6.4 NM, 100 K, 3000 RPM, 1,70KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3382,"TEM",1,"MC",11.302,1]
["1FK70617AF711KG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 6.4 NM, 100 K, 3000 RPM, 1,70KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2331,"TEM",1,"MC",10.003,1]
["1FK70617AF711SG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 6.4 NM, 100 K, 3000 RPM, 1,70KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",1492,"TEM",1,"MC",10.003,1]
["1FK70617AF711UA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 6.4 NM, 100 K, 3000 RPM, 1,70KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1897,"TEM",1,"MC",10.003,1]
["1FK70617AH711DA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 6.4 NM, 100 K, 4500 RPM, 2,03KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2585,"TEM",1,"MC",10.003,1]
["1FK70617AH711EG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 6.4 NM, 100 K, 4500 RPM, 2,03KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10%  DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2683,"TEM",1,"MC",10.003,1]
["1FK70617AH711GB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 6.4 NM, 100 K, 4500 RPM, 2,03KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2393,"TEM",1,"MC",11.302,1]
["1FK70617AH711PH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 6.4 NM, 100 K, 4500 RPM, 2,03KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2187,"TEM",1,"MC",11.302,1]
["1FK70617AH711SH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 6.4 NM, 100 K, 4500 RPM, 2,03KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",1823,"TEM",1,"MC",11.302,1]
["1FK70617AH711UB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 6.4 NM, 100 K, 4500 RPM, 2,03KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2226,"TEM",1,"MC",11.302,1]
["1FK70622AC711CA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,5 KW; UZK=600V M0=8.5NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2769,"TEM",1,"MC",9.1010000000000009,1]
["1FK70622AC711FG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,5 KW; UZK=600V M0=8.5NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2669,"TEM",1,"MC",9.1010000000000009,1]
["1FK70622AC711RA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,5 KW; UZK=600V M0=8.5NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2291,"TEM",1,"MC",9.1010000000000009,1]
["1FK70622AC711TH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,5 KW; UZK=600V M0=8.5NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",1698,"TEM",1,"MC",9.4009999999999998,1]
["1FK70622AF711BB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,9 KW; UZK=600V M0=8.5NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2703,"TEM",1,"MC",9.4,1]
["1FK70622AF711KA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,9 KW; UZK=600V M0=8.5NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 16BIT + 12BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM16DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2332,"TEM",1,"MC",9.1010000000000009,1]
["1FK70622AF711TH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,9 KW; UZK=600V M0=8.5NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",1792,"TEM",1,"MC",9.4009999999999998,1]
["1FK70622AF711UB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,9 KW; UZK=600V M0=8.5NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2117,"TEM",1,"MC",9.4009999999999998,1]
["1FK70622AH711PB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,4 KW; UZK=600V M0=8.5NM (100K); NN=4500RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2117,"TEM",1,"MC",9.5,1]
["1FK70622AH711SA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,4 KW; UZK=600V M0=8.5NM (100K); NN=4500RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1479,"TEM",1,"MC",9.1020000000000003,1]
["1FK70623BF711AB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI; PN=1,9 KW; UZK=600V M0=8,5NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VP 2048 S/R WITH C- AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2368,"TEM",1,"MC",10.9,1]
["1FK70623BF711CH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI; PN=1,9 KW; UZK=600V M0=8,5NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2988,"TEM",1,"MC",10.9,1]
["1FK70623BF711QA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI; PN=1,9 KW; UZK=600V M0=8,5NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1917,"TEM",1,"MC",10.601000000000001,1]
["1FK70632AC711BB2","SIMOTICS S SYNCHRONOUS MOTORS 1FK7-CT PN=1,9 KW; UZK=600V M0=11NM (100K); NN=2000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2796,"TEM",1,"MC",11.4,1]
["1FK70632AC711EG0","SIMOTICS S SYNCHRONOUS MOTORS 1FK7-CT PN=1,9 KW; UZK=600V M0=11NM (100K); NN=2000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2444,"TEM",1,"MC",11.101000000000001,1]
["1FK70632AC711QB1","SIMOTICS S SYNCHRONOUS MOTORS 1FK7-CT PN=1,9 KW; UZK=600V M0=11NM (100K); NN=2000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2313,"TEM",1,"MC",11.4,1]
["1FK70632AC711TA0","SIMOTICS S SYNCHRONOUS MOTORS 1FK7-CT PN=1,9 KW; UZK=600V M0=11NM (100K); NN=2000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1573,"TEM",1,"MC",11.102,1]
["1FK70632AF711BA2","SIMOTICS S SYNCHRONOUS MOTORS 1FK7-CT PN=2,3 KW; UZK=600V M0=11NM (100K); NN=3000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2493,"TEM",1,"MC",11.101000000000001,1]
["1FK70632AF711EA1","SIMOTICS S SYNCHRONOUS MOTORS 1FK7-CT PN=2,3 KW; UZK=600V M0=11NM (100K); NN=3000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2624,"TEM",1,"MC",11.101000000000001,1]
["1FK70632AF711KH0","SIMOTICS S SYNCHRONOUS MOTORS 1FK7-CT PN=2,3 KW; UZK=600V M0=11NM (100K); NN=3000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 16BIT + 12BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM16DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2551,"TEM",1,"MC",11.4,1]
["1FK70632AF711RB2","SIMOTICS S SYNCHRONOUS MOTORS 1FK7-CT PN=2,3 KW; UZK=600V M0=11NM (100K); NN=3000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2687,"TEM",1,"MC",11.4,1]
["1FK70632AF711UG2","SIMOTICS S SYNCHRONOUS MOTORS 1FK7-CT PN=2,3 KW; UZK=600V M0=11NM (100K); NN=3000RPM; NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1821,"TEM",1,"MC",11.102,1]
["1FK70632AH711PH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,4 KW; UZK=600V M0=11NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2033,"TEM",1,"MC",11.5,1]
["1FK70632AH711TA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,4 KW; UZK=600V M0=11NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1573,"TEM",1,"MC",11.102,1]
["1FK70635AC711FG2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 11NM, 100K, 2000RPM, 1,86KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3015,"TEM",1,"MC",11.503,1]
["1FK70635AF711DA2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 11NM, 100K, 3000RPM, 2,29KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2708,"TEM",1,"MC",11.503,1]
["1FK70635AF711EH8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 11NM, 100K, 3000RPM, 2,29KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10%  DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3245,"TEM",1,"MC",12.802,1]
["1FK70635AF711GG3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 11NM, 100K, 3000RPM, 2,29KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2142,"TEM",1,"MC",11.503,1]
["1FK70635AF711PB8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 11NM, 100K, 3000RPM, 2,29KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2558,"TEM",1,"MC",12.802,1]
["1FK70635AF711TA2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 11NM, 100K, 3000RPM, 2,29KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",1810,"TEM",1,"MC",11.503,1]
["1FK70635AF711UG3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 11NM, 100K, 3000RPM, 2,29KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",1925,"TEM",1,"MC",11.503,1]
["1FK70635AH711DG2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 11 NM, 100 K, 4500 RPM, 1,41KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2614,"TEM",1,"MC",11.503,1]
["1FK70635AH711FA5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 11 NM, 100 K, 4500 RPM, 1,41KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3158,"TEM",1,"MC",11.503,1]
["1FK70635AH711GH0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 11 NM, 100 K, 4500 RPM, 1,41KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2424,"TEM",1,"MC",12.802,1]
["1FK70635AH711PG8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 11 NM, 100 K, 4500 RPM, 1,41KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2136,"TEM",1,"MC",11.503,1]
["1FK70635AH711TB0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 11 NM, 100 K, 4500 RPM, 1,41KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2037,"TEM",1,"MC",12.802,1]
["1FK70644CC711AB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2,1 KW; UZK=600V M0=12NM (100K); NN=2000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2621,"TEM",1,"MC",15.7,1]
["1FK70644CC711PG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2,1 KW; UZK=600V M0=12NM (100K); NN=2000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1887,"TEM",1,"MC",15.500999999999999,1]
["1FK70644CC711SB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2,1 KW; UZK=600V M0=12NM (100K); NN=2000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2128,"TEM",1,"MC",15.701000000000001,1]
["1FK70644CF711AG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2,5 KW; UZK=600V M0=12NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2325,"TEM",1,"MC",15.401,1]
["1FK70644CF711EA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2,5 KW; UZK=600V M0=12NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2783,"TEM",1,"MC",15.401,1]
["1FK70644CF711PG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2,5 KW; UZK=600V M0=12NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1980,"TEM",1,"MC",15.500999999999999,1]
["1FK70644CF711SH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2,5 KW; UZK=600V M0=12NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2044,"TEM",1,"MC",15.701000000000001,1]
["1FK70644CH711AG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2,4 KW; UZK=600V M0=12NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2232,"TEM",1,"MC",15.401,1]
["1FK70644CH711EG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2,4 KW; UZK=600V M0=12NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2697,"TEM",1,"MC",15.401,1]
["1FK70644CH711QB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2,4 KW; UZK=600V M0=12NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2379,"TEM",1,"MC",15.7,1]
["1FK70644CH711TB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2,4 KW; UZK=600V M0=12NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2128,"TEM",1,"MC",15.701000000000001,1]
["1FK70647AF711AG5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 12.0 NM, 100 K, 3000 RPM, 2,5KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2574,"TEM",1,"MC",15.503,1]
["1FK70647AF711EB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 12.0 NM, 100 K, 3000 RPM, 2,5KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10%  DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",3250,"TEM",1,"MC",16.802,1]
["1FK70647AF711GA8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 12.0 NM, 100 K, 3000 RPM, 2,5KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2618,"TEM",1,"MC",15.503,1]
["1FK70647AF711KH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 12.0 NM, 100 K, 3000 RPM, 2,5KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2958,"TEM",1,"MC",16.802,1]
["1FK70647AF711SB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 12.0 NM, 100 K, 3000 RPM, 2,5KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2361,"TEM",1,"MC",16.802,1]
["1FK70647AF711UB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 12.0 NM, 100 K, 3000 RPM, 2,5KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2521,"TEM",1,"MC",16.802,1]
["1FK70647AH711AH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 12.0 NM, 100 K, 4500 RPM, 2,36KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3014,"TEM",1,"MC",16.802,1]
["1FK70647AH711GB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 12.0 NM, 100 K, 4500 RPM, 2,36KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2839,"TEM",1,"MC",16.802,1]
["1FK70647AH711PB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 12.0 NM, 100 K, 4500 RPM, 2,36KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2521,"TEM",1,"MC",16.802,1]
["1FK70647AH711SH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 12.0 NM, 100 K, 4500 RPM, 2,36KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2378,"TEM",1,"MC",16.802,1]
["1FK70647AH711UH3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 12.0 NM, 100 K, 4500 RPM, 2,36KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=3) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2430,"TEM",1,"MC",16.802,1]
["1FK70802AF711CB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=2,1 KW; UZK=600V M0=8NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3221,"TEM",1,"MC",10.6,1]
["1FK70802AF711KB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=2,1 KW; UZK=600V M0=8NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 16BIT + 12BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM16DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2783,"TEM",1,"MC",10.6,1]
["1FK70802AF711RG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=2,1 KW; UZK=600V M0=8NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2245,"TEM",1,"MC",10.301,1]
["1FK70802AF711UB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=2,1 KW; UZK=600V M0=8NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2266,"TEM",1,"MC",10.601000000000001,1]
["1FK70802AH711CA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=2,1 KW; UZK=600V M0=8NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2716,"TEM",1,"MC",10.301,1]
["1FK70802AH711PH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=2,1 KW; UZK=600V M0=8NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2179,"TEM",1,"MC",10.7,1]
["1FK70802AH711SG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=2,1 KW; UZK=600V M0=8NM (100K); NN=4500RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",1527,"TEM",1,"MC",10.302,1]
["1FK70805AF711AG0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 8 NM, 100 K, 3000 RPM, 2,14KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N WITHOUT HOLDING BRAKE; DEGREE OF PROTECTION IP64",2193,"TEM",1,"MC",10.003,1]
["1FK70805AF711DH5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 8 NM, 100 K, 3000 RPM, 2,14KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N WITH HOLDING BRAKE; DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2985,"TEM",1,"MC",12.502000000000001,1]
["1FK70805AF711FG5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 8 NM, 100 K, 3000 RPM, 2,14KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N WITHOUT HOLDING BRAKE; DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3007,"TEM",1,"MC",10.003,1]
["1FK70805AF711KG2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 8 NM, 100 K, 3000 RPM, 2,14KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N WITHOUT HOLDING BRAKE; DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2396,"TEM",1,"MC",10.003,1]
["1FK70805AF711TH8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 8 NM, 100 K, 3000 RPM, 2,14KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N WITH HOLDING BRAKE; DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",2196,"TEM",1,"MC",12.502000000000001,1]
["1FK70805AF711UA2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 8 NM, 100 K, 3000 RPM, 2,14KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N, WITHOUT HOLDING BRAKE; DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2014,"TEM",1,"MC",10.003,1]
["1FK70805AH711EG0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 8 NM, 100 K, 4500 RPM, 2,10KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10%  DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N WITHOUT HOLDING BRAKE; DEGREE OF PROTECTION IP64",2597,"TEM",1,"MC",10.003,1]
["1FK70805AH711GA3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 8 NM, 100 K, 4500 RPM, 2,10KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N, WITHOUT HOLDING BRAKE; DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2178,"TEM",1,"MC",10.003,1]
["1FK70805AH711PA2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 8 NM, 100 K, 4500 RPM, 2,10KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N, WITHOUT HOLDING BRAKE; DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2014,"TEM",1,"MC",10.003,1]
["1FK70805AH711SG5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 8 NM, 100 K, 4500 RPM, 2,10KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N WITHOUT HOLDING BRAKE; DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",1708,"TEM",1,"MC",10.003,1]
["1FK70805AH711UB0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 8 NM, 100 K, 4500 RPM, 2,10KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N, WITH HOLDING BRAKE; DEGREE OF PROTECTION IP64",2292,"TEM",1,"MC",12.502000000000001,1]
["1FK70812AC711BB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=2,1 KW; UZK=600V M0=12NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2975,"TEM",1,"MC",13.2,1]
["1FK70812AC711GB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=2,1 KW; UZK=600V M0=12NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 32 S/R SINGLETURN, 4096 ROTATION MULTITURN, WITH ENDAT- INTERFACE (ENCODER AM32S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2588,"TEM",1,"MC",13.2,1]
["1FK70812AC711RA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=2,1 KW; UZK=600V M0=12NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2549,"TEM",1,"MC",12.901,1]
["1FK70812AC711TH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=2,1 KW; UZK=600V M0=12NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2156,"TEM",1,"MC",13.201000000000001,1]
["1FK70812AF711BG0","SIMOTICS S SYNCHRONMOTOR 1FK7-CT PN=2,7 KW; UZK=600V M0=12NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2478,"TEM",1,"MC",12.901,1]
["1FK70812AF711KB0","SIMOTICS S SYNCHRONMOTOR 1FK7-CT PN=2,7 KW; UZK=600V M0=12NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 16BIT + 12BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM16DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2907,"TEM",1,"MC",13.2,1]
["1FK70812AF711QH2","SIMOTICS S SYNCHRONMOTOR 1FK7-CT PN=2,7 KW; UZK=600V M0=12NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2500,"TEM",1,"MC",13.2,1]
["1FK70812AF711UA2","SIMOTICS S SYNCHRONMOTOR 1FK7-CT PN=2,7 KW; UZK=600V M0=12NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2072,"TEM",1,"MC",12.901999999999999,1]
["1FK70812AH711BH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,8 KW; UZK=600V M0=12NM (100K); NN=4500RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2983,"TEM",1,"MC",13.2,1]
["1FK70812AH711SB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,8 KW; UZK=600V M0=12NM (100K); NN=4500RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2242,"TEM",1,"MC",13.201000000000001,1]
["1FK70812AH711UG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,8 KW; UZK=600V M0=12NM (100K); NN=4500RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",1892,"TEM",1,"MC",12.901999999999999,1]
["1FK70813BF711DB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI; PN=2,7 KW; UZK=600V M0=12NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",3056,"TEM",1,"MC",15.500999999999999,1]
["1FK70813BF711QB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI; PN=2,7 KW; UZK=600V M0=12NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2586,"TEM",1,"MC",15.5,1]
["1FK70827AF711EB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 14 NM, 100 K, 3000 RPM, 2,51KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10%  DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",3591,"TEM",1,"MC",19.702000000000002,1]
["1FK70827AF711SG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC, 14 NM, 100 K, 3000 RPM, 2,51KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2060,"TEM",1,"MC",17.202999999999999,1]
["1FK70832AC711CB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=2,6 KW; UZK=600V M0=16NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3546,"TEM",1,"MC",15.9,1]
["1FK70832AC711KB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=2,6 KW; UZK=600V M0=16NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 16BIT + 12BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM16DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3109,"TEM",1,"MC",15.9,1]
["1FK70832AC711RA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=2,6 KW; UZK=600V M0=16NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2656,"TEM",1,"MC",15.601000000000001,1]
["1FK70832AC711UB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=2,6 KW; UZK=600V M0=16NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2591,"TEM",1,"MC",15.901,1]
["1FK70832AF711CA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3,3 KW; UZK=600V M0=16NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3041,"TEM",1,"MC",15.601000000000001,1]
["1FK70832AF711PA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3,3 KW; UZK=600V M0=16NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2179,"TEM",1,"MC",15.701000000000001,1]
["1FK70832AF711QG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3,3 KW; UZK=600V M0=16NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2103,"TEM",1,"MC",15.601000000000001,1]
["1FK70832AF711TA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3,3 KW; UZK=600V M0=16NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",1938,"TEM",1,"MC",15.602,1]
["1FK70832AH711BB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,4 KW; UZK=600V M0=16NM (100K); NN=4500RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",3177,"TEM",1,"MC",15.9,1]
["1FK70832AH711EH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,4 KW; UZK=600V M0=16NM (100K); NN=4500RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",3127,"TEM",1,"MC",15.9,1]
["1FK70832AH711UA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=1,4 KW; UZK=600V M0=16NM (100K); NN=4500RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2179,"TEM",1,"MC",15.602,1]
["1FK70835AC711KH0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 16NM, 100K, 2000RPM, 2,62KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",3094,"TEM",1,"MC",16.501999999999999,1]
["1FK70835AF711DA8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 16NM, 100K, 3000RPM, 3,30KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3161,"TEM",1,"MC",14.003,1]
["1FK70835AF711FA5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 16NM, 100K, 3000RPM, 3,30KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3454,"TEM",1,"MC",14.003,1]
["1FK70835AF711GB0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 16NM, 100K, 3000RPM, 3,30KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2928,"TEM",1,"MC",16.501999999999999,1]
["1FK70835AF711PB2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 16NM, 100K, 3000RPM, 3,30KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2814,"TEM",1,"MC",16.501999999999999,1]
["1FK70835AF711TB0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 16NM, 100K, 3000RPM, 3,30KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2450,"TEM",1,"MC",16.501999999999999,1]
["1FK70835AF711UH3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT 16NM, 100K, 3000RPM, 3,30KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2667,"TEM",1,"MC",16.501999999999999,1]
["1FK70835AH711DB2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT16 NM, 100 K, 4500 RPM, 3,04KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3450,"TEM",1,"MC",16.501999999999999,1]
["1FK70835AH711FB0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT16 NM, 100 K, 4500 RPM, 3,04KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",3749,"TEM",1,"MC",16.501999999999999,1]
["1FK70835AH711GH3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT16 NM, 100 K, 4500 RPM, 3,04KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2884,"TEM",1,"MC",16.501999999999999,1]
["1FK70835AH711PH2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT16 NM, 100 K, 4500 RPM, 3,04KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2720,"TEM",1,"MC",16.501999999999999,1]
["1FK70835AH711TB5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT16 NM, 100 K, 4500 RPM, 3,04KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2601,"TEM",1,"MC",16.501999999999999,1]
["1FK70835AH713EH5","SIMOTICS S-1FK7 SYNCHRON-SERVO-MOTOR 1FK7 COMPACT; NATURAL COOLING NN=4500U/MIN; UZK=600V; DESIGN IMB 5 POWER CONNECT. FIXED TOWARDS BS ABSOLUTE ENCODER 2048 S/R +  4096 TURNS MULTITURN WITH ENDAT-INTERFACE (ENCODER AM2048S/R); PLAIN SHAFT TOLERANCE N WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 PAINT FINISH DE FLANSCH IP67; CUSTOMIZED VERSION CUSTOM MADE  MOTOR",3547,"TEM",1,"MC",15.6,1]
["1FK70842AC711FH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3,1 KW; UZK=600V M0=20NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3837,"TEM",1,"MC",18.600000000000001,1]
["1FK70842AC711KG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3,1 KW; UZK=600V M0=20NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 16BIT + 12BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM16DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2909,"TEM",1,"MC",18.300999999999998,1]
["1FK70842AC711RH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3,1 KW; UZK=600V M0=20NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",3279,"TEM",1,"MC",18.600000000000001,1]
["1FK70842AF711CG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3,1 KW; UZK=600V M0=20NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",3346,"TEM",1,"MC",18.300999999999998,1]
["1FK70842AF711KG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3,1 KW; UZK=600V M0=20NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 16BIT + 12BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM16DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2909,"TEM",1,"MC",18.300999999999998,1]
["1FK70842AF711RH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3,1 KW; UZK=600V M0=20NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3279,"TEM",1,"MC",18.600000000000001,1]
["1FK70842AF711UG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3,1 KW; UZK=600V M0=20NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2391,"TEM",1,"MC",18.302,1]
["1FK70843BC711CB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI; PN=3,1 KW; UZK=600V M0=20NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",3750,"TEM",1,"MC",23,1]
["1FK70843BC711FH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI; PN=3,1 KW; UZK=600V M0=20NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",3837,"TEM",1,"MC",23,1]
["1FK70843BF711AB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI; PN=3,1 KW; UZK=600V M0=20NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VP 2048 S/R WITH C- AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",3233,"TEM",1,"MC",23,1]
["1FK70843BF711CA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI; PN=3,1 KW; UZK=600V M0=20NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3339,"TEM",1,"MC",22.701000000000001,1]
["1FK70843BF711QB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI; PN=3,1 KW; UZK=600V M0=20NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2898,"TEM",1,"MC",23,1]
["1FK70854CC711AH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=3,1 KW; UZK=600V M0=22NM (100K); NN=2000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3287,"TEM",1,"MC",23.3,1]
["1FK70854CC711KA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=3,1 KW; UZK=600V M0=22NM (100K); NN=2000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 16BIT + 12BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM16DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3135,"TEM",1,"MC",23.001000000000001,1]
["1FK70854CC711QH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=3,1 KW; UZK=600V M0=22NM (100K); NN=2000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",3045,"TEM",1,"MC",23.3,1]
["1FK70854CC711TG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=3,1 KW; UZK=600V M0=22NM (100K); NN=2000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2196,"TEM",1,"MC",23.001999999999999,1]
["1FK70854CF711BH0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2 KW; UZK=600V M0=22NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",3435,"TEM",1,"MC",23.3,1]
["1FK70854CF711KA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2 KW; UZK=600V M0=22NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 16BIT + 12BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM16DQ) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",3135,"TEM",1,"MC",23.001000000000001,1]
["1FK70854CF711RB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2 KW; UZK=600V M0=22NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",3505,"TEM",1,"MC",23.3,1]
["1FK70857AF711DB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 22 NM, 100 K, 3000 RPM, 3,14KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",3824,"TEM",1,"MC",26.001999999999999,1]
["1FK70857AF711DH2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 22 NM, 100 K, 3000 RPM, 3,14KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3832,"TEM",1,"MC",26.001999999999999,1]
["1FK70857AF711GH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 22 NM, 100 K, 3000 RPM, 3,14KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",3310,"TEM",1,"MC",26.001999999999999,1]
["1FK70857AF711PB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 22 NM, 100 K, 3000 RPM, 3,14KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3237,"TEM",1,"MC",26.001999999999999,1]
["1FK70857AF711TB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 22 NM, 100 K, 3000 RPM, 3,14KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3027,"TEM",1,"MC",26.001999999999999,1]
["1FK70857AF711UH5","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FK7 HIGH DYNAMIC 22 NM, 100 K, 3000 RPM, 3,14KW NATURAL COOLING, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEGR. RESOLVER MULTI-POLE (RESOLVER P=4) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3245,"TEM",1,"MC",26.001999999999999,1]
["1FK70864CC711CG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=3,8 KW; UZK=600V M0=28NM (100K); NN=2000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3791,"TEM",1,"MC",23.001000000000001,1]
["1FK70864CC711PG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=3,8 KW; UZK=600V M0=28NM (100K); NN=2000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2929,"TEM",1,"MC",23.100999999999999,1]
["1FK70864CC711SB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=3,8 KW; UZK=600V M0=28NM (100K); NN=2000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",3092,"TEM",1,"MC",23.300999999999998,1]
["1FK70864CC711UH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=3,8 KW; UZK=600V M0=28NM (100K); NN=2000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3340,"TEM",1,"MC",23.300999999999998,1]
["1FK70864CF711EA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2 KW; UZK=600V M0=28NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3732,"TEM",1,"MC",23.001000000000001,1]
["1FK70864CF711QG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2 KW; UZK=600V M0=28NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3032,"TEM",1,"MC",23.001000000000001,1]
["1FK70864CF711SH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HD PN=2 KW; UZK=600V M0=28NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3099,"TEM",1,"MC",23.300999999999998,1]
["1FK70867AC711KA3","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 HIGH DYNAMIC, 28 NM, 100 K, 2000 RPM, 3,77KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEG. IM B5 (V1, V3) BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3698,"TEM",1,"MC",23.503,1]
["1FK70867AF711FB5","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 HIGH DYNAMIC, 28 NM, 100 K, 3000 RPM, 3,77KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEG. IM B5 (V1, V3) ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",4808,"TEM",1,"MC",26.001999999999999,1]
["1FK70867AF711FG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 HIGH DYNAMIC, 28 NM, 100 K, 3000 RPM, 3,77KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEG. IM B5 (V1, V3) ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",4117,"TEM",1,"MC",23.503,1]
["1FK70867AF711PH8","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 HIGH DYNAMIC, 28 NM, 100 K, 3000 RPM, 3,77KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEG. IM B5 (V1, V3) RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3785,"TEM",1,"MC",26.001999999999999,1]
["1FK70867AF711TG2","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 HIGH DYNAMIC, 28 NM, 100 K, 3000 RPM, 3,77KW NATURAL COOLING, POWER/SIGNAL CONNECTORS CONNECTOR CAN BE ROTATED BY 270 DEG. IM B5 (V1, V3) RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2919,"TEM",1,"MC",23.503,1]
["1FK70867SF711DB3","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 HIGH DYNAMIC, 38 NM, 100 K, 3000 RPM, 7,50KW FORCED VENTILATION, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR ROTATABLE BY 270 DEG. IM B5 (V1, V3) INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",5674,"TEM",1,"MC",30.102,1]
["1FK70867SF711KA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 HIGH DYNAMIC, 38 NM, 100 K, 3000 RPM, 7,50KW FORCED VENTILATION, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR ROTATABLE BY 270 DEG. IM B5 (V1, V3) BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",5018,"TEM",1,"MC",27.603000000000002,1]
["1FK70867SF711UG3","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FK7 HIGH DYNAMIC, 38 NM, 100 K, 3000 RPM, 7,50KW FORCED VENTILATION, IM B5 (V1, V3) POWER/SIGNAL CONNECTORS CONNECTOR ROTATABLE BY 270 DEG. IM B5 (V1, V3) RESOLVER MULTI-POLE (RESOLVER P=4) WITH DRIVE-CLIQ INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",4498,"TEM",1,"MC",27.603000000000002,1]
["1FK71002AC711EG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3 KW; UZK=600V M0=18NM (100K); NN=2000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3057,"TEM",1,"MC",17.600999999999999,1]
["1FK71002AC711QB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3 KW; UZK=600V M0=18NM (100K); NN=2000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",2848,"TEM",1,"MC",17.899999999999999,1]
["1FK71002AC711TG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3 KW; UZK=600V M0=18NM (100K); NN=2000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2006,"TEM",1,"MC",17.602,1]
["1FK71002AF711BA2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3,8 KW; UZK=600V M0=18NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3013,"TEM",1,"MC",17.600999999999999,1]
["1FK71002AF711EH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3,8 KW; UZK=600V M0=18NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3468,"TEM",1,"MC",17.899999999999999,1]
["1FK71002AF711QB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3,8 KW; UZK=600V M0=18NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",2941,"TEM",1,"MC",17.899999999999999,1]
["1FK71002AF711TA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=3,8 KW; UZK=600V M0=18NM (100K); NN=3000RPM; NATURAL COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",2092,"TEM",1,"MC",17.602,1]
["1FK71005AC711DH3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 18 NM, 100 K, 2000 RPM, 3,05KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3573,"TEM",1,"MC",22.001999999999999,1]
["1FK71005AF711AB5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,18 NM, 100 K, 3000 RPM, 3,77KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3506,"TEM",1,"MC",22.001999999999999,1]
["1FK71005AF711EH0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,18 NM, 100 K, 3000 RPM, 3,77KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10%  DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",3665,"TEM",1,"MC",22.001999999999999,1]
["1FK71005AF711FH3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,18 NM, 100 K, 3000 RPM, 3,77KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3974,"TEM",1,"MC",22.001999999999999,1]
["1FK71005AF711SB2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,18 NM, 100 K, 3000 RPM, 3,77KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",2821,"TEM",1,"MC",22.001999999999999,1]
["1FK71005AF711UB0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,18 NM, 100 K, 3000 RPM, 3,77KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",2981,"TEM",1,"MC",22.001999999999999,1]
["1FK71012AC711BB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=4,3 KW; UZK=600V M0=27NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3745,"TEM",1,"MC",23.3,1]
["1FK71012AC711EB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=4,3 KW; UZK=600V M0=27NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3875,"TEM",1,"MC",23.3,1]
["1FK71012AC711QB2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=4,3 KW; UZK=600V M0=27NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3262,"TEM",1,"MC",23.3,1]
["1FK71012AC711TA1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=4,3 KW; UZK=600V M0=27NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2506,"TEM",1,"MC",23.001999999999999,1]
["1FK71012AF711BB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=4,9 KW; UZK=600V M0=27NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",3745,"TEM",1,"MC",23.3,1]
["1FK71012AF711EB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=4,9 KW; UZK=600V M0=27NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",3875,"TEM",1,"MC",23.3,1]
["1FK71012AF711QG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=4,9 KW; UZK=600V M0=27NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2764,"TEM",1,"MC",23.001000000000001,1]
["1FK71012AF711SH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=4,9 KW; UZK=600V M0=27NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",2832,"TEM",1,"MC",23.300999999999998,1]
["1FK71013BF711CA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI PN=4,9 KW; UZK=600V M0=27NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3596,"TEM",1,"MC",25.701000000000001,1]
["1FK71015AC711DA0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,27 NM, 100 K, 2000 RPM, 4,29KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",3519,"TEM",1,"MC",21.003,1]
["1FK71015AC711EH8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,27 NM, 100 K, 2000 RPM, 4,29KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10%  DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",4273,"TEM",1,"MC",24.001999999999999,1]
["1FK71015AC711GG2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,27 NM, 100 K, 2000 RPM, 4,29KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3106,"TEM",1,"MC",21.003,1]
["1FK71015AC711PG0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,27 NM, 100 K, 2000 RPM, 4,29KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",2789,"TEM",1,"MC",21.003,1]
["1FK71015AC711UH8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,27 NM, 100 K, 2000 RPM, 4,29KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",3495,"TEM",1,"MC",24.001999999999999,1]
["1FK71015AF711DG2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 27 NM, 100 K, 3000 RPM, 4,85KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3527,"TEM",1,"MC",21.003,1]
["1FK71015AF711FG0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 27 NM, 100 K, 3000 RPM, 4,85KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",3826,"TEM",1,"MC",21.003,1]
["1FK71015AF711KB3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 27 NM, 100 K, 3000 RPM, 4,85KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3854,"TEM",1,"MC",24.001999999999999,1]
["1FK71015AF711PG5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 27 NM, 100 K, 3000 RPM, 4,85KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",2940,"TEM",1,"MC",21.003,1]
["1FK71015AF711TG3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT, 27 NM, 100 K, 3000 RPM, 4,85KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",2576,"TEM",1,"MC",21.003,1]
["1FK71032AC711AB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=5,2 KW; UZK=600V M0=36NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",3926,"TEM",1,"MC",28.8,1]
["1FK71032AC711EA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=5,2 KW; UZK=600V M0=36NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODERR 2048 S/R + 4096 UMDREHUNGEN MULTITURN, WITH ENDAT-SCHNITTSTELLE (ENCODER AM2048S/R) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3793,"TEM",1,"MC",28.501000000000001,1]
["1FK71032AC711PG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=5,2 KW; UZK=600V M0=36NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",3084,"TEM",1,"MC",28.600999999999999,1]
["1FK71032AC711SB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=5,2 KW; UZK=600V M0=36NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",3247,"TEM",1,"MC",28.800999999999998,1]
["1FK71032AF711AG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=4,4 KW; UZK=600V M0=36NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER SIN/COS 1VPP;2048 S/R W. C-AND D-SPUR (ENCODER IC2048S/R) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3335,"TEM",1,"MC",28.501000000000001,1]
["1FK71032AF711DG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=4,4 KW; UZK=600V M0=36NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 22 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER IC22DQ) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3656,"TEM",1,"MC",28.501999999999999,1]
["1FK71032AF711PH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=4,4 KW; UZK=600V M0=36NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE RESOLVER 2-POLE, WITH DRIVE CLIQ-INTERFACE PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",3495,"TEM",1,"MC",28.9,1]
["1FK71032AF711SG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=4,4 KW; UZK=600V M0=36NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",2843,"TEM",1,"MC",28.501999999999999,1]
["1FK71033BC711CG0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI PN=5,2 KW; UZK=600V M0=36NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",3928,"TEM",1,"MC",32.100999999999999,1]
["1FK71035AC711AH2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,36 NM, 100 K, 2000 RPM, 5, 24KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",4170,"TEM",1,"MC",32.002000000000002,1]
["1FK71035AC711GB0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,36 NM, 100 K, 2000 RPM, 5, 24KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",4004,"TEM",1,"MC",32.002000000000002,1]
["1FK71035AC711KH3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,36 NM, 100 K, 2000 RPM, 5, 24KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",4219,"TEM",1,"MC",32.002000000000002,1]
["1FK71035AC711SH2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,36 NM, 100 K, 2000 RPM, 5, 24KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4); PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",3534,"TEM",1,"MC",32.002000000000002,1]
["1FK71035AC711UB5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,36 NM, 100 K, 2000 RPM, 5, 24KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3939,"TEM",1,"MC",32.002000000000002,1]
["1FK71035AF711DB3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,36 NM, 100 K, 3000 RPM, 4,40KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",4474,"TEM",1,"MC",32.002000000000002,1]
["1FK71035AF711EH8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,36 NM, 100 K, 3000 RPM, 4,40KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10%  DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",4732,"TEM",1,"MC",32.002000000000002,1]
["1FK71035AF711GH8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,36 NM, 100 K, 3000 RPM, 4,40KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",4170,"TEM",1,"MC",32.002000000000002,1]
["1FK71035AF711PB5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,36 NM, 100 K, 3000 RPM, 4,40KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",3939,"TEM",1,"MC",32.002000000000002,1]
["1FK71035AF711TA0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,36 NM, 100 K, 3000 RPM, 4,40KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64",3079,"TEM",1,"MC",29.003,1]
["1FK71035AF711UG3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,36 NM, 100 K, 3000 RPM, 4,40KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER MULTI-POLE (RESOLVER P=4) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",3297,"TEM",1,"MC",29.003,1]
["1FK71052AC711CG1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=7,7 KW; UZK=600V M0=48NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65,",5100,"TEM",1,"MC",39.000999999999998,1]
["1FK71052AC711FH1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=7,7 KW; UZK=600V M0=48NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",5592,"TEM",1,"MC",39.299999999999997,1]
["1FK71052AC711RA0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=7,7 KW; UZK=600V M0=48NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP64;",4615,"TEM",1,"MC",39.000999999999998,1]
["1FK71052AC711TG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=7,7 KW; UZK=600V M0=48NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1, WITH KTY TEMPERATURESENSOR POWER CONNECTOR ROTATABLE RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",3904,"TEM",1,"MC",39.002000000000002,1]
["1FK71052AF711BB1","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=8,2 KW; UZK=600V M0=48NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 24 BIT WITH DRIVE CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65,",5229,"TEM",1,"MC",39.299999999999997,1]
["1FK71052AF711FB0","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=8,2 KW; UZK=600V M0=48NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22BIT + 12 BIT MULTITURN, WITH DRIVE-CLIQ INTERFACE (ENCODER AM22DQ) SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP64;",5584,"TEM",1,"MC",39.299999999999997,1]
["1FK71052AF711QG2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-CT PN=8,2 KW; UZK=600V M0=48NM (100K); NN=3000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER SINGLETURN 20 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS20DQI) PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",4248,"TEM",1,"MC",39.000999999999998,1]
["1FK71053BC711RH2","SIMOTICS S SYNCHRONOUS MOTOR 1FK7-HI PN=7,7 KW; UZK=600V M0=48NM (100K); NN=2000RPM; NATURAL COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 20 BIT + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM20DQI) PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE PROTECTION CLASS IP65, FLANGE ON DRIVE END IP67;",5008,"TEM",1,"MC",44.7,1]
["1FK71055AC711DG2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,48 NM, 100 K, 2000 RPM, 7,75KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",5138,"TEM",1,"MC",39.103000000000002,1]
["1FK71055AC711FA5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,48 NM, 100 K, 2000 RPM, 7,75KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",5682,"TEM",1,"MC",39.103000000000002,1]
["1FK71055AC711KA3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,48 NM, 100 K, 2000 RPM, 7,75KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",5019,"TEM",1,"MC",39.103000000000002,1]
["1FK71055AC711PG8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,48 NM, 100 K, 2000 RPM, 7,75KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",4660,"TEM",1,"MC",39.103000000000002,1]
["1FK71055AC711TB2","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,48 NM, 100 K, 2000 RPM, 7,75KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1); SHAFT WITH FITTED KEY, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP65 FLANGE ON DRIVE END IP67",4780,"TEM",1,"MC",42.101999999999997,1]
["1FK71055AF711AA5","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,48 NM, 100 K, 3000 RPM, 8,17KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 AS FLANGE IP67; PAINT FINISH RAL7016",5019,"TEM",1,"MC",39.103000000000002,1]
["1FK71055AF711DG8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,48 NM, 100 K, 3000 RPM, 8,17KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",5296,"TEM",1,"MC",39.103000000000002,1]
["1FK71055AF711FG3","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,48 NM, 100 K, 3000 RPM, 8,17KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP64; PAINT FINISH RAL7016",5487,"TEM",1,"MC",39.103000000000002,1]
["1FK71055AF711KA8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,48 NM, 100 K, 3000 RPM, 8,17KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., BASIC ABSOLUTE ENCODER 32 P/REV (ENCODER A-32) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; SHAFT WITH FITTED KEY, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",5229,"TEM",1,"MC",39.103000000000002,1]
["1FK71055AF711PH0","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,48 NM, 100 K, 3000 RPM, 8,17KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, TOLERANCE N; WITH HOLDING BRAKE DEGREE OF PROTECTION IP64",4847,"TEM",1,"MC",42.101999999999997,1]
["1FK71055AF711TG8","SIMOTICS S SYNCHRONOUS SERVOMOTORS 1FK7 COMPACT,48 NM, 100 K, 3000 RPM, 8,17KW NATURAL AIR COOLING, IM B5 (IM V1, IM V3) POWER/SIGNAL CONNECTORS CONN. CAN BE ROTATED BY 270 DEGR., RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, TOLERANCE N; W/O HOLDING BRAKE DEGREE OF PROTECTION IP65 IP67 D-END FLANGE; RAL7016 COATING; METALLIC RATING PLATE AT MOTOR",4398,"TEM",1,"MC",39.103000000000002,1]
["1FL60242AF211AB1","SIMOTICS S-1FL6 SUPPLY VOLTAGE 230V 3AC PN=0,1KW;NN=3000RPM M0=0,32NM;MN=0,32NM SHAFT HEIGHT 20MM ENCODER INCREMENTAL TTL 2500PPR WITH SHAFT KEY, TOLERANCE N WITH HOLDING BRAKE PROTECTION CLASS IP65 WITH OIL SEAL MATCHING DRIVE SINAMICS V90",627,"TEM",1,"MC",0.86,1]
["1FL60542AF210AA1","SIMOTICS S-1FL6 SUPPLY VOLTAGE 230V 3AC PN=2KW;NN=3000RPM M0=6,37NM;MN=6,37NM SHAFT HEIGHT 50MM ENCODER INCREMENTAL TTL 2500PPR WITH SHAFT KEY, TOLERANCE N WITHOUT HOLDING BRAKE PROTECTION CLASS IP65 WITH OIL SEAL MATCHING DRIVE SINAMICS V90",1058,"TEM",1,"MC",6.56,1]
["1FL60661AC610LA1","SIMOTICS S-1FL6-1FL6 SUPPLY VOLTAGE 400V 3AC PN=1.75KW;NN=2000RPM M0=11NM;MN=8.36NM SHAFT HEIGHT 65MM ENCODER ABSOLUTE 20BIT (12BIT M WITH SHAFT KEY, TOLERANCE N WITHOUT HOLDING BRAKE PROTECTION CLASS IP65 WITH OIL SEAL MATCHING DRIVE SINAMICS V70&V90",1562,"TEM",1,"MC",12.3,1]
["1FT61326AB711DL5","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 75 NM, 100 K, 1500 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE RIGHT INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, ACCURACY TOLERANCE R, W. HOLDING BRAKE VIBRATION SEVERITY GRADE R, ROTARY SHAFT SEAL (IP 67)",12506,"TEM",1,"MC",95.004000000000005,1]
["1FT61326AB713AA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 75 NM, 100 K, 1500 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) OUTGOING CONNECTOR DIRECTION AXIAL NON-DRIVE END CUSTOMIZED VERSION INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",9704,"TEM",1,"MC",85.004999999999995,1]
["1FT61326AB714EH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 75 NM, 100 K, 1500 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION AXIAL DRIVE END ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, ACCURACY TOLERANCE N, W. HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",12385,"TEM",1,"MC",95.004000000000005,1]
["1FT61326AC711DL7","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 75 NM, 100 K, 2000 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE RIGHT INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, ACCURACY TOLERANCE R, W. HOLDING BRAKE VIBRATION SEVERITY GRADE R, KEROSENE SEAL (IP 68)",12638,"TEM",1,"MC",95.004000000000005,1]
["1FT61326AC712AH1","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 75 NM, 100 K, 2000 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE LEFT INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, ACCURACY TOLERANCE N, W. HOLDING BRAKE VIBRATION SEVERITY GRADE N, GAMMA SEALING RING (IP 65)",11680,"TEM",1,"MC",95.004000000000005,1]
["1FT61326AC714DA1","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 75 NM, 100 K, 2000 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION AXIAL DRIVE END INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, GAMMA SEALING RING (IP 65)",10170,"TEM",1,"MC",85.004999999999995,1]
["1FT61326AF711AE0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 75 NM, 100 K, 3000 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE RIGHT INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); WITH FITTED KEY, ACCURACY TOLERANCE R, W. HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",11673,"TEM",1,"MC",95.004000000000005,1]
["1FT61326AF711EG1","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 75 NM, 100 K, 3000 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE RIGHT ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, GAMMA SEALING RING (IP 65)",10613,"TEM",1,"MC",85.004999999999995,1]
["1FT61326AF712DG1","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 75 NM, 100 K, 3000 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE LEFT INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, GAMMA SEALING RING (IP 65)",10170,"TEM",1,"MC",85.004999999999995,1]
["1FT61326AF714EG1","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 75 NM, 100 K, 3000 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION AXIAL DRIVE END ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, GAMMA SEALING RING (IP 65)",10613,"TEM",1,"MC",85.004999999999995,1]
["1FT61326AF718TA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 75 NM, 100 K, 3000 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR CONNECT. OF TERMINAL BOX AND SIGNAL CONNECTOR, TERMINAL BOX AXIAL DRIVE END RESOLVER 2-POLE (RESOLVER P=1); WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",8609,"TEM",1,"MC",85.504000000000005,1]
["1FT61326SC711AG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 110 NM, 100 K, 2000 RPM SEPARATE VENTILATION; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE RIGHT INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",11195,"TEM",1,"MC",91.004999999999995,1]
["1FT61326SC714AH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 110 NM, 100 K, 2000 RPM SEPARATE VENTILATION; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION AXIAL DRIVE END INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, ACCURACY TOLERANCE N, W. HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",13069,"TEM",1,"MC",101.004,1]
["1FT61326SC717TA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 110 NM, 100 K, 2000 RPM SEPARATE VENTILATION; IM B5 (IM V1, IM V3) FOR CONNECT. OF TERMINAL BOX AND SIGNAL CONNECTOR, TERMINAL BOX AXIAL NON-DRIVE END RESOLVER 2-POLE (RESOLVER P=1); WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",10100,"TEM",1,"MC",91.504000000000005,1]
["1FT61326SF714DB1","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FT6 110 NM, 100 K, 3000 REV/MIN, SEPARATE VENTILATION IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION AXIAL DRIVE END INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; WITH FITTED KEY, ACCURACY TOLERANCE N, W. HOLDING BRAKE VIBRATION SEVERITY GRADE N, GAMMA SEALING RING (IP 65)",13382,"TEM",1,"MC",101.004,1]
["1FT61326SF714DH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FT6 110 NM, 100 K, 3000 REV/MIN, SEPARATE VENTILATION IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION AXIAL DRIVE END INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, ACCURACY TOLERANCE N, W. HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",13434,"TEM",1,"MC",101.004,1]
["1FT61346AB711DG1","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 95 NM, 100 K, 1500 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE RIGHT INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, GAMMA SEALING RING (IP 65)",11425,"TEM",1,"MC",100.005,1]
["1FT61346AB712FG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 95 NM, 100 K, 1500 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE LEFT ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",12141,"TEM",1,"MC",100.005,1]
["1FT61346AB714ED3","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 95 NM, 100 K, 1500 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION AXIAL DRIVE END ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; WITH FITTED KEY, ACCURACY TOLERANCE R, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE R, DIAPHRAGM SEAL (IP 64)",12169,"TEM",1,"MC",100.005,1]
["1FT61346AC711DA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 95 NM, 100 K, 2000 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE RIGHT INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",11323,"TEM",1,"MC",100.005,1]
["1FT61346AC711TA0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 95 NM, 100 K, 2000 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE RIGHT RESOLVER 2-POLE (RESOLVER P=1); WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",9863,"TEM",1,"MC",100.005,1]
["1FT61346AC714AB1","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 95 NM, 100 K, 2000 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION AXIAL DRIVE END INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); WITH FITTED KEY, ACCURACY TOLERANCE N, W. HOLDING BRAKE VIBRATION SEVERITY GRADE N, GAMMA SEALING RING (IP 65)",12781,"TEM",1,"MC",110.004,1]
["1FT61346AC714TH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 95 NM, 100 K, 2000 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION AXIAL DRIVE END RESOLVER 2-POLE (RESOLVER P=1); PLAIN SHAFT, ACCURACY TOLERANCE N, W. HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",11738,"TEM",1,"MC",110.004,1]
["1FT61346SB714AG1","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FT6 140 NM, 100 K, 1500 REV/MIN, SEPARATE VENTILATION; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION AXIAL DRIVE END INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, GAMMA SEALING RING (IP 65)",12551,"TEM",1,"MC",106.005,1]
["1FT61346SC711DH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 140 NM, 100 K, 2000 RPM SEPARATE VENTILATION; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE RIGHT INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, ACCURACY TOLERANCE N, W. HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",14688,"TEM",1,"MC",116.004,1]
["1FT61346SC712EG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 140 NM, 100 K, 2000 RPM SEPARATE VENTILATION; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE LEFT ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",13256,"TEM",1,"MC",106.005,1]
["1FT61346SC715FG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 140 NM, 100 K, 2000 RPM SEPARATE VENTILATION; IM B5 (IM V1, IM V3) FOR CONNECT. OF TERMINAL BOX AND SIGNAL CONNECTOR, TERMINAL BOX TRAVERSE RIGHT ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",13632,"TEM",1,"MC",106.504,1]
["1FT61346SF714AH1","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FT6 140 NM, 100 K, 3000 RPM, SEPARATE VENTILATION; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION AXIAL DRIVE END INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); PLAIN SHAFT, ACCURACY TOLERANCE N, W. HOLDING BRAKE VIBRATION SEVERITY GRADE N, GAMMA SEALING RING (IP 65)",14425,"TEM",1,"MC",116.004,1]
["1FT61346SF715DA2","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FT6 140 NM, 100 K, 3000 RPM, SEPARATE VENTILATION; IM B5 (IM V1, IM V3) FOR CONNECT. OF TERMINAL BOX AND SIGNAL CONNECTOR, TERMINAL BOX TRAVERSE RIGHT INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, ROTARY SHAFT SEAL (IP 67)",13001,"TEM",1,"MC",106.504,1]
["1FT61346WD768EG1","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6; 200 NM, 100 K, 2500 REV/MIN WATER-COOLED; DESIGN IM B35; FOR TERMINAL BOX CONNECTION AND SIGNAL CONNECTOR TERMINAL BOX AXIAL DRIVE END; ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, ROTATIONAL TOLERANCE N WITHOUT HOLDING BRAKE; VIBRATION SEVERITY GRADE N GAMMA SEAL (IP 65);",12387,"TEM",1,"MC",103.504,1]
["1FT61366AB711FG1","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 115 NM, 100 K, 1500 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE RIGHT ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, GAMMA SEALING RING (IP 65)",13711,"TEM",1,"MC",117.005,1]
["1FT61366AC711AB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 115 NM, 100 K, 2000 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE RIGHT INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); WITH FITTED KEY, ACCURACY TOLERANCE N, W. HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",14146,"TEM",1,"MC",127.004,1]
["1FT61366AC711AB2","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 115 NM, 100 K, 2000 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE RIGHT INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); WITH FITTED KEY, ACCURACY TOLERANCE N, W. HOLDING BRAKE VIBRATION SEVERITY GRADE N, ROTARY SHAFT SEAL (IP 67)",14333,"TEM",1,"MC",127.004,1]
["1FT61366AC712DG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 115 NM, 100 K, 2000 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE LEFT INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",12790,"TEM",1,"MC",117.005,1]
["1FT61366AC714EB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 115 NM, 100 K, 2000 RPM NATURAL AIR COOLING; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION AXIAL DRIVE END ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; WITH FITTED KEY, ACCURACY TOLERANCE N, W. HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",14953,"TEM",1,"MC",127.004,1]
["1FT61366SB711DG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FT6 175 NM, 100 K, 1500 RPM, SEPARATE VENTILATION; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE RIGHT INCREMENTAL ENCODER 2048 P/REV (ENCODER I-2048) WITH DRIVE-CLIQ INTERFACE; PLAIN SHAFT, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",14233,"TEM",1,"MC",123.005,1]
["1FT61366SB715AB1","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FT6 175 NM, 100 K, 1500 RPM, SEPARATE VENTILATION; IM B5 (IM V1, IM V3) FOR CONNECT. OF TERMINAL BOX AND SIGNAL CONNECTOR, TERMINAL BOX TRAVERSE RIGHT INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); WITH FITTED KEY, ACCURACY TOLERANCE N, W. HOLDING BRAKE VIBRATION SEVERITY GRADE N, GAMMA SEALING RING (IP 65)",15692,"TEM",1,"MC",133.50299999999999,1]
["1FT61366SC711SG0","SIMOTICS S SYNCHRONOUS SERVOMOTOR, 1FT6 175 NM, 100 K, 2000 RPM, SEPARATE VENTILATION; IM B5 (IM V1, IM V3) FOR POWER AND SIGNAL CONNECTOR OUTGOING CONNECTOR DIRECTION TRAVERSE RIGHT RESOLVER MULTI-POLE (RESOLVER P=3); PLAIN SHAFT, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",12770,"TEM",1,"MC",123.005,1]
["1FT61366SF715AB0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 175 NM, 100 K, 3000 REV/MIN SEPARATE VENTILATION; IM B5 (IM V1, IM V3) FOR TERMINAL BOX CONNECTION AND SIGNAL POINT TERMINAL BOX CROSSWISE RIGHT INCREM. ENCODER, SIN/COS 1 VPP 2048 P/REV (ENCODER I-2048); WITH FITTED KEY, ACCURACY TOLERANCE N, W. HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",15590,"TEM",1,"MC",133.50299999999999,1]
["1FT61366SF717FH0","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6 175 NM, 100 K, 3000 REV/MIN SEPARATE VENTILATION; IM B5 (IM V1, IM V3) FOR TERMINAL BOX CONNECTION AND SIGNAL POINT TERMINAL BOX AXIAL NON-DRIVE END ABSOLUTE ENCODER 2048 P/REV (ENCODER A-2048) WITH DRIVE-CLIQ INTERFACE; PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, ACCURACY TOLERANCE N, W. HOLDING BRAKE VIBRATION SEVERITY GRADE N, DIAPHRAGM SEAL (IP 64)",16927,"TEM",1,"MC",133.50299999999999,1]
["1FT61386WD766EK4","SIMOTICS S SYNCHRONOUS SERVOMOTOR 1FT6; 300 NM, 100 K, 2500 REV/MIN; WATER-COOLED; DESIGN IM B35; FOR TERMINAL BOX CONNECTION AND SIGNAL CONNECTOR TERMINAL BOX CROSSWISE LEFT; ABSOLUTE ENCODER ENDAT 2048 P/REV (ENCODER A-2048); PERFORMANCE REDUCTION BY 10% DUE TO ABSOLUTE ENCODER; PLAIN SHAFT, ROTATIONAL TOLERANCE R WITHOUT HOLDING BRAKE; VIBRATION SEVERITY GRADE R GAMMA SEAL (IP 65);",15036,"TEM",1,"MC",137.50399999999999,1]
["1FT70345AK701BA1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=2NM (100K) NN=6000RPM, PN=0,88KW NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",3192,"TEM",1,"MC",3.9039999999999999,1]
["1FT70345AK701FA1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=2NM (100K) NN=6000RPM, PN=0,88KW NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4038,"TEM",1,"MC",3.9039999999999999,1]
["1FT70345AK711BG2","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=2NM (100K) NN=6000RPM, PN=0,88KW NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",3272,"TEM",1,"MC",3.9039999999999999,1]
["1FT70345AK711DK1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=2NM (100K) NN=6000RPM, PN=0,88KW NATURAL AIR COOLING, FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",3432,"TEM",1,"MC",3.9039999999999999,1]
["1FT70345AK711MB1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=2NM (100K) NN=6000RPM, PN=0,88KW NATURAL AIR COOLING, IM B5, STANDARD BRIDE (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4241,"TEM",1,"MC",4.2030000000000003,1]
["1FT70365AK701CG0","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=3NM (100K) NN=6000RPM, PN=1,07KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",4001,"TEM",1,"MC",5.1040000000000001,1]
["1FT70365AK711FA1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=3NM (100K) NN=6000RPM, PN=1,07KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4177,"TEM",1,"MC",5.1040000000000001,1]
["1FT70365AK711FA5","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=3NM (100K) NN=6000RPM, PN=1,07KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",4413,"TEM",1,"MC",5.1040000000000001,1]
["1FT70425AF701DG3","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=3NM (100K) NN=3000RPM, PN=0,85KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",3512,"TEM",1,"MC",4.7039999999999997,1]
["1FT70425AF701MH0","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=3NM (100K) NN=3000RPM, PN=0,85KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE (COMPACT) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",4377,"TEM",1,"MC",5.4029999999999996,1]
["1FT70425AF711CK1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=3NM (100K) NN=3000RPM, PN=0,85KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4298,"TEM",1,"MC",4.7039999999999997,1]
["1FT70425AF711FD4","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=3NM (100K) NN=3000RPM, PN=0,85KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",4534,"TEM",1,"MC",4.7039999999999997,1]
["1FT70425AF711MG0","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=3NM (100K) NN=3000RPM, PN=0,85KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",3691,"TEM",1,"MC",4.7039999999999997,1]
["1FT70425AK701FB3","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=3NM (100K) NN=6000RPM, PN=1,26KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",4963,"TEM",1,"MC",5.4029999999999996,1]
["1FT70425AK711CA5","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=3NM (100K) NN=6000RPM, PN=1,26KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",4374,"TEM",1,"MC",4.7039999999999997,1]
["1FT70425AK711FH2","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=3NM (100K) NN=6000RPM, PN=1,26KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",4984,"TEM",1,"MC",5.4029999999999996,1]
["1FT70441AF701NH1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=5NM (100K) NN=3000RPM, PN=1,35KW NATURAL AIR COOLING; POWER CONNECTOR ROTATABLE VIBRATION SEVERITY GRADE A PROTECTION CLASS IP 65; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE (COMPACT) WITH KTY TEMPERATURE SENSOR INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N",3034,"TEM",1,"MC",7.9,1]
["1FT70445AF701CG3","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=5NM (100K) NN=3000RPM, PN=1,35KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",4560,"TEM",1,"MC",7.3040000000000003,1]
["1FT70445AF701MB2","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=5NM (100K) NN=3000RPM, PN=1,35KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE (COMPACT) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",4915,"TEM",1,"MC",8.0030000000000001,1]
["1FT70445AF711CB4","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=5NM (100K) NN=3000RPM, PN=1,35KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",5343,"TEM",1,"MC",8.0030000000000001,1]
["1FT70445AF711FD5","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=5NM (100K) NN=3000RPM, PN=1,35KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",4977,"TEM",1,"MC",7.3040000000000003,1]
["1FT70445AF711NA3","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=5NM (100K) NN=3000RPM, PN=1,35KW NATURAL AIR COOLING; FRAME SIZE IM B5 (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",3454,"TEM",1,"MC",7.3040000000000003,1]
["1FT70445AK701MK2","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=5NM (100K) NN=6000RPM, PN=1,41KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE (COMPACT) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",4389,"TEM",1,"MC",7.3040000000000003,1]
["1FT70445AK711FA5","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=5NM (100K) NN=6000RPM, PN=1,41KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",4817,"TEM",1,"MC",7.3040000000000003,1]
["1FT70445AK711NG2","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=5NM (100K) NN=6000RPM, PN=1,41KW NATURAL AIR COOLING; FRAME SIZE IM B5 (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",3475,"TEM",1,"MC",7.3040000000000003,1]
["1FT70465AF701DB0","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=7NM (100K) NN=3000RPM, PN=1,76KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",4711,"TEM",1,"MC",10.103,1]
["1FT70465AF701NH1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=7NM (100K) NN=3000RPM, PN=1,76KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE (COMPACT) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4387,"TEM",1,"MC",10.103,1]
["1FT70465AF711DA3","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=7NM (100K) NN=3000RPM, PN=1,76KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",4180,"TEM",1,"MC",9.4039999999999999,1]
["1FT70465AF711NA4","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=7NM (100K) NN=3000RPM, PN=1,76KW NATURAL AIR COOLING; FRAME SIZE IM B5 (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",3857,"TEM",1,"MC",9.4039999999999999,1]
["1FT70465AH701DH0","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=7NM (100K) NN=4500RPM, PN=1,32KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",4711,"TEM",1,"MC",10.103,1]
["1FT70465AH711DB0","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=7NM (100K) NN=4500RPM, PN=1,32KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",4711,"TEM",1,"MC",10.103,1]
["1FT70465AH711NB1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=7NM (100K) NN=4500RPM, PN=1,32KW NATURAL AIR COOLING; FRAME SIZE IM B5 (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4387,"TEM",1,"MC",10.103,1]
["1FT70621AK711NG1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=6NM (100K) NN=6000RPM, PN=2,13KW NATURAL AIR COOLING; POWER CONNECTOR ROTATABLE VIBRATION SEVERITY GRADE A PROTECTION CLASS IP 65; FRAME SIZE IMB 5 (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACCURACY TOLERANCE N",2466,"TEM",1,"MC",7.1,1]
["1FT70625AF701FH0","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=6NM (100K) NN=3000RPM, PN=1,70KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5226,"TEM",1,"MC",8.5030000000000001,1]
["1FT70625AF711CB2","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=6NM (100K) NN=3000RPM, PN=1,70KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",5322,"TEM",1,"MC",8.5030000000000001,1]
["1FT70625AF711FG0","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=6NM (100K) NN=3000RPM, PN=1,70KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",4432,"TEM",1,"MC",7.2039999999999997,1]
["1FT70625AK701DG1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=6NM (100K) NN=6000RPM, PN=2,13KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",3763,"TEM",1,"MC",7.2039999999999997,1]
["1FT70625AK711FA0","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=6NM (100K) NN=6000RPM, PN=2,13KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",4432,"TEM",1,"MC",7.2039999999999997,1]
["1FT70625WK711DG4","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=10NM (100K) NN=6000RPM, PN=5,80KW WATER-COOLED; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",4565,"TEM",1,"MC",11.103999999999999,1]
["1FT70641AF711NG1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=9NM (100K) NN=3000RPM, PN=2,39KW NATURAL AIR COOLING; POWER CONNECTOR ROTATABLE VIBRATION SEVERITY GRADE A PROTECTION CLASS IP 65; FRAME SIZE IMB 5 (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACCURACY TOLERANCE N",2767,"TEM",1,"MC",9.6999999999999993,1]
["1FT70645AF701BK3","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=9NM (100K) NN=3000RPM, PN=2,39KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",4326,"TEM",1,"MC",9.8040000000000003,1]
["1FT70645AF701DB1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=9NM (100K) NN=3000RPM, PN=2,39KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4982,"TEM",1,"MC",11.103,1]
["1FT70645AF711BK5","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=9NM (100K) NN=3000RPM, PN=2,39KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",4503,"TEM",1,"MC",9.8040000000000003,1]
["1FT70645AF711DG2","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=9NM (100K) NN=3000RPM, PN=2,39KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",4268,"TEM",1,"MC",9.8040000000000003,1]
["1FT70645AF711ML1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=9NM (100K) NN=3000RPM, PN=2,39KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",5472,"TEM",1,"MC",11.103,1]
["1FT70645AK701FG1","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=9NM (100K) NN=6000RPM, PN=2,59KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4953,"TEM",1,"MC",9.8040000000000003,1]
["1FT70645AK711DD3","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=9NM (100K) NN=6000RPM, PN=2,59KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",4406,"TEM",1,"MC",9.8040000000000003,1]
["1FT70645AK711NK5","SIMOTICS S SYNCHRONOUS MOTOR 1FT7, M0=9NM (100K) NN=6000RPM, PN=2,59KW NATURAL AIR COOLING; FRAME SIZE IM B5 (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",4162,"TEM",1,"MC",9.8040000000000003,1]
["1FT70645WK701CG2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=16NM (100K) NN=6000RPM, PN=8,90KW WATER-COOLED; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",5594,"TEM",1,"MC",13.804,1]
["1FT70657SH701CA1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=14NM (100K) NN=4500RPM, PN=5,20KW SEPARATE VENTILATION; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",5875,"TEM",1,"MC",19.103999999999999,1]
["1FT70665AF701BK4","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=12NM (100K) NN=3000RPM, PN=2,92KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",4733,"TEM",1,"MC",12.404,1]
["1FT70665AF701NH0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=12NM (100K) NN=3000RPM, PN=2,92KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE (COMPACT) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",4775,"TEM",1,"MC",13.702999999999999,1]
["1FT70665AF711CB2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=12NM (100K) NN=3000RPM, PN=2,92KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",6056,"TEM",1,"MC",13.702999999999999,1]
["1FT70665AF711FB1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=12NM (100K) NN=3000RPM, PN=2,92KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6057,"TEM",1,"MC",13.702999999999999,1]
["1FT70665AH701CB0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=12NM (100K) NN=4500RPM, PN=2,55KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5880,"TEM",1,"MC",13.702999999999999,1]
["1FT70665AH711MG1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=12NM (100K) NN=4500RPM, PN=2,55KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4831,"TEM",1,"MC",12.404,1]
["1FT70665WH701FG2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=20NM (100K) NN=4500RPM, PN=9,10KW WATER-COOLED; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",5984,"TEM",1,"MC",16.404,1]
["1FT70677SH701CB1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=17NM (100K) NN=4500RPM, PN=6,10KW SEPARATE VENTILATION; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6975,"TEM",1,"MC",24.402999999999999,1]
["1FT70685AF701BG4","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=15NM (100K) NN=3000RPM, PN=3,42KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",4883,"TEM",1,"MC",16.404,1]
["1FT70685AF701DK2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=15NM (100K) NN=3000RPM, PN=3,42KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",5046,"TEM",1,"MC",16.404,1]
["1FT70685AF711CA1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=15NM (100K) NN=3000RPM, PN=3,42KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",5492,"TEM",1,"MC",16.404,1]
["1FT70685AF711FG3","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=15NM (100K) NN=3000RPM, PN=3,42KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",5631,"TEM",1,"MC",16.404,1]
["1FT70685AF711NH0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=15NM (100K) NN=3000RPM, PN=3,42KW NATURAL AIR COOLING; FRAME SIZE IM B5 (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5084,"TEM",1,"MC",17.702999999999999,1]
["1FT70821AF701DH1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=13NM (100K) NN=3000RPM, PN=3,24KW NATURAL AIR COOLING; POWER CONNECTOR ROTATABLE VIBRATION SEVERITY GRADE A PROTECTION CLASS IP 65; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE, ACCURACY TOLERANCE N",3880,"TEM",1,"MC",17.100000000000001,1]
["1FT70825AC701CB2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=13NM (100K) NN=2000RPM, PN=2,39KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",5850,"TEM",1,"MC",17.202999999999999,1]
["1FT70825AC701NA0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=13NM (100K) NN=2000RPM, PN=2,39KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE (COMPACT) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",3671,"TEM",1,"MC",14.103999999999999,1]
["1FT70825AC711DA5","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=13NM (100K) NN=2000RPM, PN=2,39KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",4424,"TEM",1,"MC",14.103999999999999,1]
["1FT70825AC711NA2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=13NM (100K) NN=2000RPM, PN=2,39KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",3847,"TEM",1,"MC",14.103999999999999,1]
["1FT70825AF701FG1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=13NM (100K) NN=3000RPM, PN=3,24KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING  BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4953,"TEM",1,"MC",14.103999999999999,1]
["1FT70825AF711MA1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=13NM (100K) NN=3000RPM, PN=3,24KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4521,"TEM",1,"MC",14.103999999999999,1]
["1FT70825AF711MG1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=13NM (100K) NN=3000RPM, PN=3,24KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING  BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4521,"TEM",1,"MC",14.103999999999999,1]
["1FT70825AH701MH1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=13NM (100K) NN=4500RPM, PN=3,77KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE (COMPACT) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",5419,"TEM",1,"MC",17.202999999999999,1]
["1FT70825WC701NG1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=21NM (100K) NN=2000RPM, PN=4,40KW WATER-COOLED; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE (COMPACT) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING  BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",4409,"TEM",1,"MC",20.803999999999998,1]
["1FT70841AF711CH1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=20NM (100K) NN=3000RPM, PN=4,56KW NATURAL AIR COOLING; POWER CONNECTOR ROTATABLE VIBRATION SEVERITY GRADE A PROTECTION CLASS IP 65; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE, ACCURACY TOLERANCE N",5108,"TEM",1,"MC",24,1]
["1FT70845AC701BA2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=20NM (100K) NN=2000RPM, PN=3,54KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",4939,"TEM",1,"MC",20.904,1]
["1FT70845AC701FG3","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=20NM (100K) NN=2000RPM, PN=3,54KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING  BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",5764,"TEM",1,"MC",20.904,1]
["1FT70845AC711BG2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=20NM (100K) NN=2000RPM, PN=3,54KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING  BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",4939,"TEM",1,"MC",20.904,1]
["1FT70845AC711DG0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=20NM (100K) NN=2000RPM, PN=3,54KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING  BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",4844,"TEM",1,"MC",20.904,1]
["1FT70845AC711NB4","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=20NM (100K) NN=2000RPM, PN=3,54KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",5573,"TEM",1,"MC",24.003,1]
["1FT70845AF701DB0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=20NM (100K) NN=3000RPM, PN=4,55KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5741,"TEM",1,"MC",24.003,1]
["1FT70845AF711CE3","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=20NM (100K) NN=3000RPM, PN=4,55KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",6738,"TEM",1,"MC",24.003,1]
["1FT70845AF711DB0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=20NM (100K) NN=3000RPM, PN=4,55KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5741,"TEM",1,"MC",24.003,1]
["1FT70845AF711FH5","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=20NM (100K) NN=3000RPM, PN=4,55KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",6838,"TEM",1,"MC",24.003,1]
["1FT70845AH701CG0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=20NM (100K) NN=4500RPM, PN=4,82KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING  BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5529,"TEM",1,"MC",20.904,1]
["1FT70845AH701NH0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=20NM (100K) NN=4500RPM, PN=4,82KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE (COMPACT) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5321,"TEM",1,"MC",24.003,1]
["1FT70845SC701CH0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=27NM (100K) NN=2000RPM, PN=5,00KW SEPARATE VENTILATION; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",7068,"TEM",1,"MC",28.202999999999999,1]
["1FT70845SC701MB3","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=27NM (100K) NN=2000RPM, PN=5,00KW SEPARATE VENTILATION; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE (COMPACT) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",6871,"TEM",1,"MC",28.103000000000002,1]
["1FT70845SH711ND4","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=27NM (100K) NN=4500RPM, PN=9,90KW SEPARATE VENTILATION; FRAME SIZE IMB 5 (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",5476,"TEM",1,"MC",25.004000000000001,1]
["1FT70845WF711FA0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=35NM (100K) NN=3000RPM, PN=11,00KW WATER-COOLED; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6250,"TEM",1,"MC",27.603999999999999,1]
["1FT70845WH711CA2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=35NM (100K) NN=4500RPM, PN=14,60KW WATER-COOLED; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",6346,"TEM",1,"MC",27.603999999999999,1]
["1FT70845WH711DH1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=35NM (100K) NN=4500RPM, PN=14,60KW WATER-COOLED; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6479,"TEM",1,"MC",30.702999999999999,1]
["1FT70861AF701BH1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=28NM (100K) NN=3000RPM, PN=5,65KW NATURAL AIR COOLING; POWER CONNECTOR ROTATABLE VIBRATION SEVERITY GRADE A PROTECTION CLASS IP 65; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE, ACCURACY TOLERANCE N",5080,"TEM",1,"MC",30.6,1]
["1FT70861AH701NH1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=28NM (100K) NN=4500RPM, PN=4,71KW NATURAL AIR COOLING; POWER CONNECTOR ROTATABLE VIBRATION SEVERITY GRADE A PROTECTION CLASS IP 65; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE (COMPACT) WITH KTY TEMPERATURE SENSOR INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE, ACCURACY TOLERANCE N",4739,"TEM",1,"MC",34.9,1]
["1FT70865AC701CG4","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=28NM (100K) NN=2000RPM, PN=4,71KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING  BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",6754,"TEM",1,"MC",27.603999999999999,1]
["1FT70865AC701MB0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=28NM (100K) NN=2000RPM, PN=4,71KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE (COMPACT) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",7048,"TEM",1,"MC",30.702999999999999,1]
["1FT70865AC711CB1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=28NM (100K) NN=2000RPM, PN=4,71KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7495,"TEM",1,"MC",30.702999999999999,1]
["1FT70865AC711FD2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=28NM (100K) NN=2000RPM, PN=4,71KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",6917,"TEM",1,"MC",27.603999999999999,1]
["1FT70865AF701BG0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=28NM (100K) NN=3000RPM, PN=5,65KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING  BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5736,"TEM",1,"MC",27.603999999999999,1]
["1FT70865AF701DH5","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=28NM (100K) NN=3000RPM, PN=5,65KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",7046,"TEM",1,"MC",30.702999999999999,1]
["1FT70865AF711BH2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=28NM (100K) NN=3000RPM, PN=5,65KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",6810,"TEM",1,"MC",30.702999999999999,1]
["1FT70865AF711DH2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=28NM (100K) NN=3000RPM, PN=5,65KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",6890,"TEM",1,"MC",30.702999999999999,1]
["1FT70865AF711FK4","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=28NM (100K) NN=3000RPM, PN=5,65KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",6993,"TEM",1,"MC",27.603999999999999,1]
["1FT70865AH711BG4","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=28NM (100K) NN=4500RPM, PN=4,71KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING  BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",5989,"TEM",1,"MC",31.904,1]
["1FT70865AH711FH0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=28NM (100K) NN=4500RPM, PN=4,71KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",7479,"TEM",1,"MC",35.003,1]
["1FT70865SF701BB0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=36NM (100K) NN=3000RPM, PN=9,10KW SEPARATE VENTILATION; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",7276,"TEM",1,"MC",39.103000000000002,1]
["1FT70865SF711MA1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=36NM (100K) NN=3000RPM, PN=9,10KW SEPARATE VENTILATION; FRAME SIZE IMB 5 (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6887,"TEM",1,"MC",36.003999999999998,1]
["1FT70865SH711CA1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=36NM (100K) NN=4500RPM, PN=11,80KW SEPARATE VENTILATION; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7239,"TEM",1,"MC",36.103999999999999,1]
["1FT70865WC711DL4","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=2000RPM, PN=10,50KW WATER-COOLED; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",7765,"TEM",1,"MC",37.302999999999997,1]
["1FT70865WF711DH4","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=3000RPM, PN=15,40KW WATER-COOLED; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",7608,"TEM",1,"MC",37.302999999999997,1]
["1FT70865WH711DG2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=4500RPM, PN=20,30KW WATER-COOLED; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING  BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",6634,"TEM",1,"MC",34.204000000000001,1]
["1FT70877SF701NA4","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=48NM (100K) NN=3000RPM, PN=10,40KW SEPARATE VENTILATION; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE (COMPACT) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",7085,"TEM",1,"MC",43.003999999999998,1]
["1FT70877SH702BA0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=48NM (100K) NN=4500RPM, PN=10,80KW SEPARATE VENTILATION; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE LEFT ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) WITH FITTED KEY, ACCURACY TOLERANCE N, W/O HOLDING BRAKE VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",7174,"TEM",1,"MC",43.003999999999998,1]
["1FT70877WH711DK5","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=61NM (100K) NN=4500RPM, PN=21,70KW WATER-COOLED; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",7745,"TEM",1,"MC",41.103999999999999,1]
["1FT71025AB701BH0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=30NM (100K) NN=1500RPM, PN=4,08KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",6440,"TEM",1,"MC",30.702999999999999,1]
["1FT71025AB701FA1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=30NM (100K) NN=1500RPM, PN=4,08KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6368,"TEM",1,"MC",26.204000000000001,1]
["1FT71025AB711CB3","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=30NM (100K) NN=1500RPM, PN=4,08KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",7360,"TEM",1,"MC",30.702999999999999,1]
["1FT71025AB711MA0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=30NM (100K) NN=1500RPM, PN=4,08KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",5840,"TEM",1,"MC",26.204000000000001,1]
["1FT71025AC701FA4","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=30NM (100K) NN=2000RPM, PN=5,03KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",6524,"TEM",1,"MC",26.204000000000001,1]
["1FT71025AC711NA3","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=30NM (100K) NN=2000RPM, PN=5,03KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",5241,"TEM",1,"MC",26.204000000000001,1]
["1FT71025AF701DA3","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=30NM (100K) NN=3000RPM, PN=6,28KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",5662,"TEM",1,"MC",26.204000000000001,1]
["1FT71025AF711CA1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=30NM (100K) NN=3000RPM, PN=6,28KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6288,"TEM",1,"MC",26.204000000000001,1]
["1FT71025AF711DH2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=30NM (100K) NN=3000RPM, PN=6,28KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",6696,"TEM",1,"MC",30.702999999999999,1]
["1FT71025AF711NB1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=30NM (100K) NN=3000RPM, PN=6,28KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6195,"TEM",1,"MC",30.702999999999999,1]
["1FT71025WF711BG1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=3000RPM, PN=14,30KW WATER-COOLED; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",6164,"TEM",1,"MC",36.704000000000001,1]
["1FT71051AC711CH1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=2000RPM, PN=7,96KW NATURAL AIR COOLING; POWER CONNECTOR ROTATABLE VIBRATION SEVERITY GRADE A PROTECTION CLASS IP 65; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N",6889,"TEM",1,"MC",48.8,1]
["1FT71055AB701DA3","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=1500RPM, PN=6,60KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",7188,"TEM",1,"MC",44.304000000000002,1]
["1FT71055AB701MH1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=1500RPM, PN=6,60KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE (COMPACT) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",8475,"TEM",1,"MC",48.802999999999997,1]
["1FT71055AB711CB1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=1500RPM, PN=6,60KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",8827,"TEM",1,"MC",48.802999999999997,1]
["1FT71055AB711FB2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=1500RPM, PN=6,60KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",8986,"TEM",1,"MC",48.802999999999997,1]
["1FT71055AC701CA5","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=2000RPM, PN=7,96KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",8049,"TEM",1,"MC",44.304000000000002,1]
["1FT71055AC701FA5","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=2000RPM, PN=7,96KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",8130,"TEM",1,"MC",44.304000000000002,1]
["1FT71055AC711BB1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=2000RPM, PN=7,96KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",8062,"TEM",1,"MC",48.802999999999997,1]
["1FT71055AC711CL5","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=2000RPM, PN=7,96KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",9221,"TEM",1,"MC",48.802999999999997,1]
["1FT71055AC711MG0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=2000RPM, PN=7,96KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",7366,"TEM",1,"MC",44.304000000000002,1]
["1FT71055AF701FG0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=3000RPM, PN=8,80KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",7798,"TEM",1,"MC",44.304000000000002,1]
["1FT71055AF711CA1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=3000RPM, PN=8,80KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7814,"TEM",1,"MC",44.304000000000002,1]
["1FT71055AF711DD4","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=3000RPM, PN=8,80KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",7444,"TEM",1,"MC",44.304000000000002,1]
["1FT71055AF711FG4","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=3000RPM, PN=8,80KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",8050,"TEM",1,"MC",44.304000000000002,1]
["1FT71055AF711NH0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=50NM (100K) NN=3000RPM, PN=8,80KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",7625,"TEM",1,"MC",48.802999999999997,1]
["1FT71055SC711CA1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=65NM (100K) NN=2000RPM, PN=11,70KW SEPARATE VENTILATION; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",8455,"TEM",1,"MC",50.103999999999999,1]
["1FT71055SF701BG1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=65NM (100K) NN=3000RPM, PN=15,10KW SEPARATE VENTILATION; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",7690,"TEM",1,"MC",50.003999999999998,1]
["1FT71055SF704CB1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=65NM (100K) NN=3000RPM, PN=15,10KW SEPARATE VENTILATION; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL DRIVE END ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9468,"TEM",1,"MC",54.603000000000002,1]
["1FT71055SF711CL1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=65NM (100K) NN=3000RPM, PN=15,10KW SEPARATE VENTILATION; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9627,"TEM",1,"MC",54.603000000000002,1]
["1FT71055SF713CB0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=65NM (100K) NN=3000RPM, PN=15,10KW SEPARATE VENTILATION; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL NON-DRIVE END ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",9372,"TEM",1,"MC",54.603000000000002,1]
["1FT71055SF714MH1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=65NM (100K) NN=3000RPM, PN=15,10KW SEPARATE VENTILATION; FRAME SIZE IMB 5 (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL DRIVE END ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9116,"TEM",1,"MC",54.503,1]
["1FT71055WC701BH4","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=90NM (100K) NN=2000RPM, PN=18,80KW WATER-COOLED; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",8859,"TEM",1,"MC",59.402999999999999,1]
["1FT71055WF701FH1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=90NM (100K) NN=3000RPM, PN=24,80KW WATER-COOLED; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9548,"TEM",1,"MC",59.402999999999999,1]
["1FT71055WF713BH1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=90NM (100K) NN=3000RPM, PN=24,80KW WATER-COOLED; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL NON-DRIVE END ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",8703,"TEM",1,"MC",59.402999999999999,1]
["1FT71085AB701DB3","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=70NM (100K) NN=1500RPM, PN=9,58KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",10213,"TEM",1,"MC",63.603000000000002,1]
["1FT71085AB701DG0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=70NM (100K) NN=1500RPM, PN=9,58KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",9045,"TEM",1,"MC",59.103999999999999,1]
["1FT71085AB711DD1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=70NM (100K) NN=1500RPM, PN=9,58KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9301,"TEM",1,"MC",59.103999999999999,1]
["1FT71085AB711NB1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=70NM (100K) NN=1500RPM, PN=9,58KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9733,"TEM",1,"MC",63.603000000000002,1]
["1FT71085AC701CG1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=70NM (100K) NN=2000RPM, PN=10,50KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9826,"TEM",1,"MC",59.103999999999999,1]
["1FT71085AC701FG2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=70NM (100K) NN=2000RPM, PN=10,50KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",9986,"TEM",1,"MC",59.103999999999999,1]
["1FT71085AC711CG1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=70NM (100K) NN=2000RPM, PN=10,50KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9826,"TEM",1,"MC",59.103999999999999,1]
["1FT71085AC711DH5","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=70NM (100K) NN=2000RPM, PN=10,50KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",10389,"TEM",1,"MC",63.603000000000002,1]
["1FT71085AC711MK4","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=70NM (100K) NN=2000RPM, PN=10,50KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 65",9790,"TEM",1,"MC",59.103999999999999,1]
["1FT71085AF701BH0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=70NM (100K) NN=3000RPM, PN=6,28KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",9978,"TEM",1,"MC",63.603000000000002,1]
["1FT71085AF701FB1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=70NM (100K) NN=3000RPM, PN=6,28KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",10919,"TEM",1,"MC",63.603000000000002,1]
["1FT71085AF711CG2","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=70NM (100K) NN=3000RPM, PN=6,28KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 67",9906,"TEM",1,"MC",59.103999999999999,1]
["1FT71085AF711FK3","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=70NM (100K) NN=3000RPM, PN=6,28KW NATURAL AIR COOLING; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 22 BITS MULTI TURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM-22-DQ) CONNECTOR ROTATABLE PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE R VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 64",10124,"TEM",1,"MC",59.103999999999999,1]
["1FT71085SC701CA0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=91NM (100K) NN=2000RPM, PN=15,30KW SEPARATE VENTILATION; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR ROTATABLE ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",10371,"TEM",1,"MC",64.103999999999999,1]
["1FT71085SC711NH1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=91NM (100K) NN=2000RPM, PN=15,30KW SEPARATE VENTILATION; FRAME SIZE IMB 5 (IM V1, IM V3) (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR POWER CONNECTOR ROTATABLE INCREM. ENCODER SIN/COS 1VSS 2048 S/R (ENCODER I-2048) CONNECTOR ROTATABLE PLAIN SHAFT, WITH HOLDING BRAKE; ACCURACY TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",10375,"TEM",1,"MC",68.503,1]
["1FT71085SF704BB0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=91NM (100K) NN=3000RPM, PN=18,80KW SEPARATE VENTILATION; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 0 POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL DRIVE END ABSOLUTE VALUE ENCODER SINGLETURN 24 BIT WITH DRIVE-CLIQ INTERFACE (ENCODER AS24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",10619,"TEM",1,"MC",68.503,1]
["1FT71085SF713CB0","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=91NM (100K) NN=3000RPM, PN=18,80KW SEPARATE VENTILATION; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL NON-DRIVE END ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; WITH HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 64",11384,"TEM",1,"MC",68.602999999999994,1]
["1FT71085SF717CG1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=91NM (100K) NN=3000RPM, PN=18,80KW SEPARATE VENTILATION; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) FOR CONNECT. OF TERMINAL BOXAND  SIGNAL CONNECTOR, TERMINALBOX AXIAL NON-DRIVE END ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) PLAIN SHAFT, W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",10467,"TEM",1,"MC",64.602999999999994,1]
["1FT71085WC715MA5","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=125NM (100K) NN=2000RPM, PN=26,20KW WATER-COOLED; FRAME SIZE IMB 5 (1FT6 COMPATIBLE) WITH KTY TEMPERATURE SENSOR FOR CONNECT. OF TERMINAL BOXAND  SIGNAL CONNECTOR, TERMINALBOX TRAVERSE RIGHT ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER A-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A+R, DEGREE OF PROTECTION IP 67",10351,"TEM",1,"MC",69.203000000000003,1]
["1FT71085WF711CA1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=125NM (100K) NN=3000RPM, PN=34,20KW WATER-COOLED; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONTRAVERSE RIGHT ABSOLUTE ENCODER 24 BITS + 12 BIT MULTITURN WITH DRIVE-CLIQ INTERFACE (ENCODER AM24DQI) SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",10467,"TEM",1,"MC",68.703999999999994,1]
["1FT71085WF714DA1","SIMOTICS S SYNCHRON. MOTOR 1FT7, M0=125NM (100K) NN=3000RPM, PN=34,20KW WATER-COOLED; FRAME SIZE IMB 5 (IM V1, IM V3) FLANGE 1 (1FT6 COMPATIBLE) POWER CONNECTOR OUTGOING CONNECTOR DIRECTIONAXIAL DRIVE END INCREMENTAL ENCODER 2048 S/R WITH DRIVE-CLIQ INTERFACE (ENCODER I-2048) CONNECTOR ROTATABLE SHAFT WITH FITTED KEY; W/O HOLDING BRAKE; ACC. TOLERANCE N VIBRATION SEVERITY GRADE A, DEGREE OF PROTECTION IP 65",9782,"TEM",1,"MC",68.703999999999994,1]
["1PH80831AF000BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 2,8KW, 18NM, 7,5A,346V 1750RPM, 3,3KW, 18NM, 7,5A,398V 2000RPM, 3,7KW, 18NM, 7,6A,447V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",3147,"TEM",1,"MC",32,1]
["1PH80831AF202CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 3,5KW,22NM, 8,9A, 357V 1750RPM, 4,0KW,22NM, 8,7A, 416V 2000RPM, 4,6KW,22NM, 8,7A, 457V WATER COOLING DEGREE OF PROTECTION IP65 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",3657,"TEM",1,"MC",36,1]
["1PH80831DF000BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 2,8KW, 18NM, 7,5A,346V 1750RPM, 3,3KW, 18NM, 7,5A,398V 2000RPM, 3,7KW, 18NM, 7,6A,447V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4555,"TEM",1,"MC",32,1]
["1PH80831DF102BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 2,8KW,18NM, 7,5A, 346V 1750RPM, 3,3KW,18NM, 7,5A, 398V 2000RPM, 3,7KW,72NM, 7,6A, 447V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4555,"TEM",1,"MC",32,1]
["1PH80831DG120BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 3,7KW,18NM, 11,6A,293V 2300RPM, 4,1KW,17NM, 11,3A,332V 2650RPM, 4,6KW,17NM, 11,2A,376V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4707,"TEM",1,"MC",32,1]
["1PH80831DM101DA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 3000RPM, 4,1KW,13NM, 13,6A,298V 3300RPM, 4,5KW,13NM, 13,5A,327V 3600RPM, 4,9KW, 13NM, 14A, 355V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE SR/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4820,"TEM",1,"MC",32,1]
["1PH80831HF001BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 2,8KW, 18NM, 7,5A,346V 1750RPM, 3,3KW, 18NM, 7,5A,398V 2000RPM, 3,7KW, 18NM, 7,6A,447V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",3536,"TEM",1,"MC",32,1]
["1PH80831HF122BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 2,8KW,18NM, 7,5A, 346V 1750RPM, 3,3KW,18NM, 7,5A, 398V 2000RPM, 3,7KW,72NM, 7,6A, 447V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",3688,"TEM",1,"MC",32,1]
["1PH80831HN100CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 4500RPM, 4,8KW,10NM, 17A,300V 5000RPM, 5,3KW,10NM, 17A, 335V 5500RPM, 5,5KW, 11NM,16,5A,350V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",3731,"TEM",1,"MC",32,1]
["1PH80831JF122BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 2,8KW,18NM, 7,5A, 346V 1750RPM, 3,3KW,18NM, 7,5A, 398V 2000RPM, 3,7KW,72NM, 7,6A, 447V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4100,"TEM",1,"MC",32,1]
["1PH80831MF002BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 2,8KW, 18NM, 7,5A,346V 1750RPM, 3,3KW, 18NM, 7,5A,398V 2000RPM, 3,7KW, 18NM, 7,6A,447V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",3861,"TEM",1,"MC",32,1]
["1PH80831TF001LA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 2,8KW, 18NM, 7,5A,346V 1750RPM, 3,3KW, 18NM, 7,5A,398V 2000RPM, 3,7KW, 18NM, 7,6A,447V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 512 S/R WITHOUT ND-END AT TERMINAL BOX (ENCODER IC512S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4625,"TEM",1,"MC",32,1]
["1PH80871AF220BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 4,6KW,29NM, 13,7A,316V 1750RPM, 5,4KW,29NM, 13,7A,358V 2000RPM, 6,1KW,29NM, 13,7A,402V WATER COOLING DEGREE OF PROTECTION IP65 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",3776,"TEM",1,"MC",44,1]
["1PH80871AM120CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 3000RPM, 4,8KW,15NM, 17,3A,284V 3300RPM, 5,2KW,15NM, 17,1A,303V 3600RPM, 5,7KW,15NM, 17,1A,355V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",3661,"TEM",1,"MC",32,1]
["1PH80871DF022BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 3,7KW, 24NM, 10A,336V 1750RPM, 4,3KW, 23NM, 10A,396V 2000RPM, 4,9KW, 23NM, 10A,435V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4873,"TEM",1,"MC",39,1]
["1PH80871DG020LA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 4,9KW,23NM, 14,1A,320V 2300RPM, 5,4KW,22NM, 13,7A,353V 2650RPM, 6,0KW,22NM, 13,6A,390V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5420,"TEM",1,"MC",39,1]
["1PH80871DN100DB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 4500RPM, 5,8KW,12NM, 19,5A,315V 5000RPM, 6,5KW,12NM, 19,5A,335V 5500RPM, 6,9KW, 12NM, 19A, 370V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE SR/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4987,"TEM",1,"MC",32,1]
["1PH80871HF100CC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 3,7KW,24NM, 10A, 336V 1750RPM, 4,3KW,23NM, 10A, 396V 2000RPM, 4,9KW,23NM, 10A, 435V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",3898,"TEM",1,"MC",39,1]
["1PH80871HF202BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 4,6KW,29NM, 13,7A,316V 1750RPM, 5,4KW,29NM, 13,7A,358V 2000RPM, 6,1KW,29NM, 13,7A,402V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4013,"TEM",1,"MC",44,1]
["1PH80871HM102CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 3000RPM, 4,8KW,15NM, 17,3A,284V 3300RPM, 5,2KW,15NM, 17,1A,303V 3600RPM, 5,7KW,15NM, 17,1A,355V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",3898,"TEM",1,"MC",32,1]
["1PH80871JF122CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 3,7KW,24NM, 10A, 336V 1750RPM, 4,3KW,23NM, 10A, 396V 2000RPM, 4,9KW,23NM, 10A, 435V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4461,"TEM",1,"MC",39,1]
["1PH80871JM102BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 3000RPM, 4,8KW,15NM, 17,3A,284V 3300RPM, 5,2KW,15NM, 17,1A,303V 3600RPM, 5,7KW,15NM, 17,1A,355V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4115,"TEM",1,"MC",32,1]
["1PH80871SF023LG1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 3,7KW, 24NM, 10A,336V 1750RPM, 4,3KW, 23NM, 10A,396V 2000RPM, 4,9KW, 23NM, 10A,435V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 19 BIT WITHOUT COMMUTATING POSITION (ENCODER IN19DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN HOLLOW-SHAFT BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",8195,"TEM",1,"MC",41.5,1]
["1PH81011AF021CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM,3,7KW, 24NM, 12,5A,265V 2000RPM, 4,3KW,22NM, 12,5A,304V 2000RPM, 4,7KW, 22NM,12,5A,343V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",3775,"TEM",1,"MC",42,1]
["1PH81011AF132CC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 3,7KW,24NM,12,5A, 265V 1750RPM, 4,3KW,23NM,12,5A, 304V 2000RPM, 4,7KW,22NM,12,5A, 343V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4014,"TEM",1,"MC",42,1]
["1PH81011AF232BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 5KW, 32NM, 12,8A, 357V 1750RPM, 5,8KW,32NM, 12,8A,400V 2000RPM, 6,6KW,32NM, 12,5A,450V WATER COOLING DEGREE OF PROTECTION IP65 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4210,"TEM",1,"MC",51,1]
["1PH81011DF031BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM,3,7KW, 24NM, 12,5A,265V 2000RPM, 4,3KW,22NM, 12,5A,304V 2000RPM, 4,7KW, 22NM,12,5A,343V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5226,"TEM",1,"MC",42,1]
["1PH81011HF002BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM,3,7KW, 24NM, 12,5A,265V 2000RPM, 4,3KW,22NM, 12,5A,304V 2000RPM, 4,7KW, 22NM,12,5A,343V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",3774,"TEM",1,"MC",42,1]
["1PH81011HF222BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 5KW, 32NM, 12,8A, 357V 1750RPM, 5,8KW,32NM, 12,8A,400V 2000RPM, 6,6KW,32NM, 12,5A,450V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4360,"TEM",1,"MC",51,1]
["1PH81011JF100CC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 3,7KW,24NM,12,5A, 265V 1750RPM, 4,3KW,23NM,12,5A, 304V 2000RPM, 4,7KW,22NM,12,5A, 343V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4381,"TEM",1,"MC",42,1]
["1PH81011JF202CC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 5KW, 32NM, 12,8A, 357V 1750RPM, 5,8KW,32NM, 12,8A,400V 2000RPM, 6,6KW,32NM, 12,5A,450V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4772,"TEM",1,"MC",51,1]
["1PH81011MS001BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR Y2000RPM, 4,9KW,23NM,13,2A,328V D5000RPM, 4,9 KW,9NM,13,5A,360V Y1500RPM, 3,7KW,24NM,13,2A,253V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4099,"TEM",1,"MC",42,1]
["1PH81031AD130CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 3,7KW, 35NM, 10A, 333V 1150RPM, 4,3KW, 36NM, 10A, 380V 1350RPM, 4,7KW,33NM, 9,7A, 423V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4121,"TEM",1,"MC",51,1]
["1PH81031AF121BF1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 5,5KW,35NM,13,1A, 368V 1750RPM, 6,3KW,34NM,13,5A, 412V 2000RPM, 7KW, 33NM, 12,7A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",3688,"TEM",1,"MC",51,1]
["1PH81031AF220BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 7,1KW,45NM, 19,7A,317V 1750RPM, 8,2KW,45NM, 19,7A,364V 2000RPM, 9,4KW,45NM, 19,7A,411V WATER COOLING DEGREE OF PROTECTION IP65 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4101,"TEM",1,"MC",60,1]
["1PH81031AM020CE1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 3000RPM, 8,4KW, 27NM,25,7A,297V 3300RPM, 9,3KW,27NM, 25,7A,326V 3600RPM, 10KW, 27NM, 25,4A,355V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",3883,"TEM",1,"MC",51,1]
["1PH81031DD032BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 3,7KW,35NM, 10,0A,333V 1150RPM, 4,3KW,36NM,10,0A, 380V 1350RPM, 4,7KW,33NM, 9,7A, 423V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5333,"TEM",1,"MC",51,1]
["1PH81031DF020CC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 5,5KW,35NM, 13,1A,342V 1750RPM, 6,3KW,34NM, 13,5A,412V 2000RPM, 7,0KW,33NM, 12,7A,460V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5290,"TEM",1,"MC",51,1]
["1PH81031DF032DA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 5,5KW,35NM, 13,1A,342V 1750RPM, 6,3KW,34NM, 13,5A,412V 2000RPM, 7,0KW,33NM, 12,7A,460V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: SR/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5599,"TEM",1,"MC",51,1]
["1PH81031DG021BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 7,0KW, 31NM, 17A, 345V 2300RPM, 7,5KW,33NM, 17,5A,400V 2650RPM, 8,0KW, 29NM, 16A, 434V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5095,"TEM",1,"MC",51,1]
["1PH81031DG030DH1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 7,0KW, 31NM, 17A, 345V 2300RPM, 7,5KW,33NM, 17,5A,400V 2650RPM, 8,0KW, 29NM, 16A, 434V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: SR/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5599,"TEM",1,"MC",51,1]
["1PH81031DG230CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 9,5KW,45NM, 23,8A,343V 2300RPM, 10,9KW,45NM,23,8A,390V 2650RPM, 12,5KW,45NM,23,5A,454V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5942,"TEM",1,"MC",60,1]
["1PH81031FF020CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 5,5KW,35NM, 13,1A,342V 1750RPM, 6,3KW,34NM, 13,5A,412V 2000RPM, 7,0KW,33NM, 12,7A,460V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",6200,"TEM",1,"MC",51,1]
["1PH81031HD022BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 3,7KW,35NM, 10,0A,333V 1150RPM, 4,3KW,36NM,10,0A, 380V 1350RPM, 4,7KW,33NM, 9,7A, 423V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4076,"TEM",1,"MC",51,1]
["1PH81031HF102CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 5,5KW,35NM,13,1A, 368V 1750RPM, 6,3KW,34NM,13,5A, 412V 2000RPM, 7KW, 33NM, 12,7A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4076,"TEM",1,"MC",51,1]
["1PH81031HF202BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 7,1KW,45NM, 19,7A,317V 1750RPM, 8,2KW,45NM, 19,7A,364V 2000RPM, 9,4KW,45NM, 19,7A,411V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4295,"TEM",1,"MC",60,1]
["1PH81031HG022BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 7,0KW, 31NM, 17A, 345V 2300RPM, 7,5KW,33NM, 17,5A,400V 2650RPM, 8,0KW, 29NM, 16A, 434V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4076,"TEM",1,"MC",51,1]
["1PH81031JD120BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 3,7KW, 35NM, 10A, 333V 1150RPM, 4,3KW, 36NM, 10A, 380V 1350RPM, 4,7KW,33NM, 9,7A, 423V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4488,"TEM",1,"MC",51,1]
["1PH81031JF102BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 5,5KW,35NM,13,1A, 368V 1750RPM, 6,3KW,34NM,13,5A, 412V 2000RPM, 7KW, 33NM, 12,7A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4293,"TEM",1,"MC",51,1]
["1PH81031JF122BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 5,5KW,35NM,13,1A, 368V 1750RPM, 6,3KW,34NM,13,5A, 412V 2000RPM, 7KW, 33NM, 12,7A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4488,"TEM",1,"MC",51,1]
["1PH81031MD121BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 3,7KW, 35NM, 10A, 333V 1150RPM, 4,3KW, 36NM, 10A, 380V 1350RPM, 4,7KW,33NM, 9,7A, 423V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4401,"TEM",1,"MC",51,1]
["1PH81031MM130LC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 3000RPM, 8,4KW, 27NM,25,7A,297V 3300RPM, 9,3KW,27NM, 25,7A,326V 3600RPM, 10KW, 27NM, 25,4A,355V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5153,"TEM",1,"MC",51,1]
["1PH81051AF002LA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM,7,0KW,45NM, 17,5A, 348V 1750RPM,8,0KW,44NM, 17,5A, 400V 2000RPM,9,0KW,43NM, 17,0A, 453V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4196,"TEM",1,"MC",65,1]
["1PH81051AF130CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 7KW, 45NM, 17,5A, 348V 1750RPM, 8KW, 44NM, 17,5A, 400V 2000RPM, 9KW, 43NM, 17A, 453V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4311,"TEM",1,"MC",65,1]
["1PH81051AF222CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 11KW,70NM, 28,5A, 340V 1750RPM, 12,5KW,68NM,28,5A,380V 2000RPM, 14KW,67NM, 27,5A, 426V WATER COOLING DEGREE OF PROTECTION IP65 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4600,"TEM",1,"MC",74,1]
["1PH81051DF001CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM,7,0KW,45NM, 17,5A, 348V 1750RPM,8,0KW,44NM, 17,5A, 400V 2000RPM,9,0KW,43NM, 17,0A, 453V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5285,"TEM",1,"MC",65,1]
["1PH81051DF022CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM,7,0KW,45NM, 17,5A, 348V 1750RPM,8,0KW,44NM, 17,5A, 400V 2000RPM,9,0KW,43NM, 17,0A, 453V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5481,"TEM",1,"MC",65,1]
["1PH81051DF131BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 7KW, 45NM, 17,5A, 348V 1750RPM, 8KW, 44NM, 17,5A, 400V 2000RPM, 9KW, 43NM, 17A, 453V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5524,"TEM",1,"MC",65,1]
["1PH81051HF031BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM,7,0KW,45NM, 17,5A, 348V 1750RPM,8,0KW,44NM, 17,5A, 400V 2000RPM,9,0KW,43NM, 17,0A, 453V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4505,"TEM",1,"MC",65,1]
["1PH81051HF100CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 7KW, 45NM, 17,5A, 348V 1750RPM, 8KW, 44NM, 17,5A, 400V 2000RPM, 9KW, 43NM, 17A, 453V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4267,"TEM",1,"MC",65,1]
["1PH81051HF230CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 11KW,70NM, 28,5A, 340V 1750RPM, 12,5KW,68NM,28,5A,380V 2000RPM, 14KW,67NM, 27,5A, 426V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5227,"TEM",1,"MC",74,1]
["1PH81051JF120CC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 7KW, 45NM, 17,5A, 348V 1750RPM, 8KW, 44NM, 17,5A, 400V 2000RPM, 9KW, 43NM, 17A, 453V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4874,"TEM",1,"MC",65,1]
["1PH81051JF220BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 11KW,70NM, 28,5A, 340V 1750RPM, 12,5KW,68NM,28,5A,380V 2000RPM, 14KW,67NM, 27,5A, 426V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5206,"TEM",1,"MC",74,1]
["1PH81051MF130DB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 7KW, 45NM, 17,5A, 348V 1750RPM, 8KW, 44NM, 17,5A, 400V 2000RPM, 9KW, 43NM, 17A, 453V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: SR/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5095,"TEM",1,"MC",65,1]
["1PH81053FF022AA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM,7,0KW,45NM, 17,5A, 348V 1750RPM,8,0KW,44NM, 17,5A, 400V 2000RPM,9,0KW,43NM, 17,0A, 453V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD VIBRATION SEVERITY GRADE A; SHAFT A.FLANGE ACCURACY GR.N TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5848,"TEM",1,"MC",65,1]
["1PH81071AD130BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 6,3KW,60NM, 17,5A,307V 1150RPM, 7,2KW,60NM, 17,5A,348V 1350RPM, 8KW, 57NM, 17A, 400V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4258,"TEM",1,"MC",73,1]
["1PH81071AF122BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 9KW, 57NM, 23,5A, 330V 1750RPM, 10KW, 55NM, 22A, 380V 2000RPM, 11KW,53NM, 21,5A, 428V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4020,"TEM",1,"MC",73,1]
["1PH81071AF220BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 14KW,89NM, 43,4A, 277V 1750RPM, 15,5KW,85NM, 42A, 314V 2000RPM, 18KW,86NM, 42,6A, 363V WATER COOLING DEGREE OF PROTECTION IP65 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4752,"TEM",1,"MC",83,1]
["1PH81071AF232BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 14KW,89NM, 43,4A, 277V 1750RPM, 15,5KW,85NM, 42A, 314V 2000RPM, 18KW,86NM, 42,6A, 363V WATER COOLING DEGREE OF PROTECTION IP65 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4990,"TEM",1,"MC",83,1]
["1PH81071DD001CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 6,3KW,60NM,17,5A, 307V 1150RPM, 7,2KW,60NM,17,5A, 348V 1350RPM, 8,0KW, 57NM, 17A, 400V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5427,"TEM",1,"MC",73,1]
["1PH81071DD031BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 6,3KW,60NM,17,5A, 307V 1150RPM, 7,2KW,60NM,17,5A, 348V 1350RPM, 8,0KW, 57NM, 17A, 400V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5665,"TEM",1,"MC",73,1]
["1PH81071DF002BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 9,0KW,57NM,23,5A, 330V 1750RPM, 10,0KW,55NM, 22A, 380V 2000RPM, 11KW,53NM, 21,5A, 428V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5232,"TEM",1,"MC",73,1]
["1PH81071DF022HA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 9,0KW,57NM,23,5A, 330V 1750RPM, 10,0KW,55NM, 22A, 380V 2000RPM, 11KW,53NM, 21,5A, 428V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5337,"TEM",1,"MC",73,1]
["1PH81071DF120CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 9KW, 57NM, 23,5A, 330V 1750RPM, 10KW, 55NM, 22A, 380V 2000RPM, 11KW,53NM, 21,5A, 428V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5622,"TEM",1,"MC",73,1]
["1PH81071DG000CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 10,5KW,50NM, 26A, 355V 2300RPM, 12KW,50NM,26A, 406V 2650RPM, 13KW, 47NM, 24A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5427,"TEM",1,"MC",73,1]
["1PH81071DG031BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 10,5KW,50NM, 26A, 355V 2300RPM, 12KW,50NM,26A, 406V 2650RPM, 13KW, 47NM, 24A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5665,"TEM",1,"MC",73,1]
["1PH81071DM021LA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 3000RPM, 12KW, 38NM, 38A, 294V 3300RPM, 13KW, 38NM, 38A, 326V 3600RPM, 14KW,37NM, 37,5A, 355V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5940,"TEM",1,"MC",73,1]
["1PH81071FF230BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 14KW,89NM, 43,4A, 277V 1750RPM, 15,5KW,85NM, 42A, 314V 2000RPM, 18KW,86NM, 42,6A, 363V WATER COOLING DEGREE OF PROTECTION IP65 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7308,"TEM",1,"MC",83,1]
["1PH81071FG030CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 10,5KW,50NM, 26A, 355V 2300RPM, 12KW,50NM,26A, 406V 2650RPM, 13KW, 47NM, 24A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6771,"TEM",1,"MC",73,1]
["1PH81071HD122GB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 6,3KW,60NM, 17,5A,307V 1150RPM, 7,2KW,60NM, 17,5A,348V 1350RPM, 8KW, 57NM, 17A, 400V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4123,"TEM",1,"MC",73,1]
["1PH81071HF101DH1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 9KW, 57NM, 23,5A, 330V 1750RPM, 10KW, 55NM, 22A, 380V 2000RPM, 11KW,53NM, 21,5A, 428V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: SR/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4478,"TEM",1,"MC",73,1]
["1PH81071HF132BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 9KW, 57NM, 23,5A, 330V 1750RPM, 10KW, 55NM, 22A, 380V 2000RPM, 11KW,53NM, 21,5A, 428V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4647,"TEM",1,"MC",73,1]
["1PH81071HF232BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 14KW,89NM, 43,4A, 277V 1750RPM, 15,5KW,85NM, 42A, 314V 2000RPM, 18KW,86NM, 42,6A, 363V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5379,"TEM",1,"MC",83,1]
["1PH81071JD022GA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 6,3KW,60NM,17,5A, 307V 1150RPM, 7,2KW,60NM,17,5A, 348V 1350RPM, 8,0KW, 57NM, 17A, 400V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4535,"TEM",1,"MC",73,1]
["1PH81071JF001BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 9,0KW,57NM,23,5A, 330V 1750RPM, 10,0KW,55NM, 22A, 380V 2000RPM, 11KW,53NM, 21,5A, 428V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4625,"TEM",1,"MC",73,1]
["1PH81071JF130CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 9KW, 57NM, 23,5A, 330V 1750RPM, 10KW, 55NM, 22A, 380V 2000RPM, 11KW,53NM, 21,5A, 428V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5254,"TEM",1,"MC",73,1]
["1PH81071JF222CC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 14KW,89NM, 43,4A, 277V 1750RPM, 15,5KW,85NM, 42A, 314V 2000RPM, 18KW,86NM, 42,6A, 363V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5747,"TEM",1,"MC",83,1]
["1PH81071MF020LA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 9,0KW,57NM,23,5A, 330V 1750RPM, 10,0KW,55NM, 22A, 380V 2000RPM, 11KW,53NM, 21,5A, 428V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5246,"TEM",1,"MC",73,1]
["1PH81071MM221BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 3000RPM, 18KW, 57NM, 60A, 294V 3300RPM, 20KW, 58NM, 60A, 326V 3600RPM, 21KW, 56NM, 59A, 355V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5466,"TEM",1,"MC",83,1]
["1PH81071SM000MA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 3000RPM, 12KW, 38NM, 38A, 294V 3300RPM, 13KW, 38NM, 38A, 326V 3600RPM, 14KW,37NM, 37,5A, 355V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 19 BIT WITH COMMUTATING POSITION (ENCODER IN19DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: HIGH PERFORMANCE VIBRATION SEVERITY GRADE SPECIAL/B SHAFT AND FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7622,"TEM",1,"MC",73,1]
["1PH81311AF102CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 11KW, 70NM, 24A, 360V 1750RPM, 13KW, 71NM, 24A, 416V 2000RPM, 15KW, 72NM, 24A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD VIBRATION SEVERITY GRADE S/A; SHAFT A.FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4178,"TEM",1,"MC",89,1]
["1PH81311CS023MC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM,14,6KW, 70NM, 39A, 302V 5000RPM,14,6KW, 28NM, 40A, 360V 1500RPM, 11KW, 70NM, 39A, 227V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 256 S/R WITHOUT ND-END AT TERMINAL BOX (ENCODER IN256S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN HOLLOW-SHAFT BEARING: HIGH PERFORMANCE VIBRATION SEVERITY GRADE SPECIAL/B SHAFT AND FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",9093,"TEM",1,"MC",91.5,1]
["1PH81311DB101GA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 400RPM, 2,9KW, 69NM, 9A, 272V 500RPM, 3,6KW, 69NM, 9A, 328V 600RPM, 4,3KW, 68NM, 9A, 384V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5106,"TEM",1,"MC",89,1]
["1PH81311DF101CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 11KW, 70NM, 24A, 360V 1750RPM, 13KW, 71NM, 24A, 416V 2000RPM, 15KW, 72NM, 24A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5586,"TEM",1,"MC",89,1]
["1PH81311DG230BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 18KW, 86NM, 40A, 352V 2300RPM, 20KW, 83NM, 39A, 400V 2650RPM, 23KW, 83NM, 39A, 458V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",6701,"TEM",1,"MC",105,1]
["1PH81311HF022BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 11KW, 70NM, 24A, 360V 1750RPM, 13KW, 71NM, 24A, 416V 2000RPM, 15KW, 72NM, 24A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4611,"TEM",1,"MC",89,1]
["1PH81311HF130BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 11KW, 70NM, 24A, 360V 1750RPM, 13KW, 71NM, 24A, 416V 2000RPM, 15KW, 72NM, 24A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4914,"TEM",1,"MC",89,1]
["1PH81311HF230CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 15KW, 96NM, 30A, 380V 1750RPM, 17KW, 93NM, 30A, 425V 2000RPM, 18,5KW, 88NM, 30A,460V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5877,"TEM",1,"MC",105,1]
["1PH81311JF122CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 11KW, 70NM, 24A, 360V 1750RPM, 13KW, 71NM, 24A, 416V 2000RPM, 15KW, 72NM, 24A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5217,"TEM",1,"MC",89,1]
["1PH81311JF202BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 15KW, 96NM, 30A, 380V 1750RPM, 17KW, 93NM, 30A, 425V 2000RPM, 18,5KW, 88NM, 30A,460V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5552,"TEM",1,"MC",105,1]
["1PH81311MF022BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 11KW, 70NM, 24A, 360V 1750RPM, 13KW, 71NM, 24A, 416V 2000RPM, 15KW, 72NM, 24A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4936,"TEM",1,"MC",89,1]
["1PH81311SF023LA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 11KW, 70NM, 24A, 360V 1750RPM, 13KW, 71NM, 24A, 416V 2000RPM, 15KW, 72NM, 24A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 19 BIT WITHOUT COMMUTATION POSITION (ENCODER IN19DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN HOLLOW-SHAFT BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",9114,"TEM",1,"MC",91.5,1]
["1PH81312DF200BA1","SIMOTICS M COMPACT SYNCHRONOUS MOTOR 1500RPM,17,6KW,112NM, 40A, 326V 1750RPM,20,4KW,112NM, 40A, 377V 2000RPM,23,2KW,111NM, 39A, 427V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",10277,"TEM",1,"MC",102,1]
["1PH81312FF221BA1","SIMOTICS M COMPACT SYNCHRONOUS MOTOR 1500RPM,17,6KW,112NM, 40A, 326V 1750RPM,20,4KW,112NM, 40A, 377V 2000RPM,23,2KW,111NM, 39A, 427V WATER COOLING DEGREE OF PROTECTION IP65 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",11426,"TEM",1,"MC",102,1]
["1PH81331AD032BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 12KW, 115NM, 30A, 319V 1150RPM,13,5KW,112NM, 29A, 361V 1350RPM, 15KW, 106NM, 28A, 417V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4650,"TEM",1,"MC",106,1]
["1PH81331AF002BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 15KW, 96NM, 34A, 342V 1750RPM,17,5KW, 96NM, 34A, 392V 2000RPM, 20KW, 96NM, 34A, 445V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4108,"TEM",1,"MC",106,1]
["1PH81331AF130CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 15KW, 96NM, 34A, 342V 1750RPM,17,5KW, 96NM, 34A, 392V 2000RPM, 20KW, 96NM, 34A, 445V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD VIBRATION SEVERITY GRADE S/A; SHAFT A.FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",4845,"TEM",1,"MC",106,1]
["1PH81331AG022BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 20KW, 96NM, 45A, 350V 2300RPM,22,5KW, 93NM, 44A, 400V 2650RPM, 24KW, 86NM, 41A, 456V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4347,"TEM",1,"MC",106,1]
["1PH81331DD000LA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 12KW, 115NM, 30A, 319V 1150RPM,13,5KW,112NM, 29A, 361V 1350RPM, 15KW, 106NM, 28A, 417V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6062,"TEM",1,"MC",106,1]
["1PH81331DD122BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 12KW, 115NM, 30A, 319V 1150RPM,13,5KW,112NM, 29A, 361V 1350RPM, 15KW, 106NM, 28A, 417V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5754,"TEM",1,"MC",106,1]
["1PH81331DF020DG1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 15KW, 96NM, 34A, 342V 1750RPM,17,5KW, 96NM, 34A, 392V 2000RPM, 20KW, 96NM, 34A, 445V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: SR/A, SHAFT AND FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",6019,"TEM",1,"MC",106,1]
["1PH81331DF031BE1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 15KW, 96NM, 34A, 342V 1750RPM,17,5KW, 96NM, 34A, 392V 2000RPM, 20KW, 96NM, 34A, 445V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R POWER CONNECTOR (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6058,"TEM",1,"MC",106,1]
["1PH81331DF121BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 15KW, 96NM, 34A, 342V 1750RPM,17,5KW, 96NM, 34A, 392V 2000RPM, 20KW, 96NM, 34A, 445V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5754,"TEM",1,"MC",106,1]
["1PH81331DG002BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 20KW, 96NM, 45A, 350V 2300RPM,22,5KW, 93NM, 44A, 400V 2650RPM, 24KW, 86NM, 41A, 456V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5516,"TEM",1,"MC",106,1]
["1PH81331DG031BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 20KW, 96NM, 45A, 350V 2300RPM,22,5KW, 93NM, 44A, 400V 2650RPM, 24KW, 86NM, 41A, 456V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",6058,"TEM",1,"MC",106,1]
["1PH81331DG221BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 22KW, 105NM, 52A, 336V 2300RPM, 25KW, 104NM, 52A, 373V 2650RPM, 28KW, 101NM, 50A, 427V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",6560,"TEM",1,"MC",123,1]
["1PH81331FF102BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 15KW, 96NM, 34A, 342V 1750RPM,17,5KW, 96NM, 34A, 392V 2000RPM, 20KW, 96NM, 34A, 445V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6426,"TEM",1,"MC",106,1]
["1PH81331HD101BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 12KW, 115NM, 30A, 319V 1150RPM,13,5KW,112NM, 29A, 361V 1350RPM, 15KW, 106NM, 28A, 417V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4497,"TEM",1,"MC",106,1]
["1PH81331HD130CC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 12KW, 115NM, 30A, 319V 1150RPM,13,5KW,112NM, 29A, 361V 1350RPM, 15KW, 106NM, 28A, 417V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5234,"TEM",1,"MC",106,1]
["1PH81331HF101BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 15KW, 96NM, 34A, 342V 1750RPM,17,5KW, 96NM, 34A, 392V 2000RPM, 20KW, 96NM, 34A, 445V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",4497,"TEM",1,"MC",106,1]
["1PH81331HF131BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 15KW, 96NM, 34A, 342V 1750RPM,17,5KW, 96NM, 34A, 392V 2000RPM, 20KW, 96NM, 34A, 445V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5039,"TEM",1,"MC",106,1]
["1PH81331HF232BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 17KW, 108NM, 38A, 345V 1750RPM, 19,5KW, 106NM, 38A, 40 2000RPM, 22,5KW, 107NM, 38A, 45 WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5845,"TEM",1,"MC",123,1]
["1PH81331HG131BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 20KW, 96NM, 45A, 350V 2300RPM,22,5KW, 93NM, 44A, 400V 2650RPM, 24KW, 86NM, 41A, 456V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5039,"TEM",1,"MC",106,1]
["1PH81331JF122BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 15KW, 96NM, 34A, 342V 1750RPM,17,5KW, 96NM, 34A, 392V 2000RPM, 20KW, 96NM, 34A, 445V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5147,"TEM",1,"MC",106,1]
["1PH81331JF222BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 17KW, 108NM, 38A, 345V 1750RPM, 19,5KW, 106NM, 38A, 40 2000RPM, 22,5KW, 107NM, 38A, 45 WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5953,"TEM",1,"MC",123,1]
["1PH81331MD020CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 12KW, 115NM, 30A, 319V 1150RPM,13,5KW,112NM, 29A, 361V 1350RPM, 15KW, 106NM, 28A, 417V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5256,"TEM",1,"MC",106,1]
["1PH81331MG000BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 20KW, 96NM, 45A, 350V 2300RPM,22,5KW, 93NM, 44A, 400V 2650RPM, 24KW, 86NM, 41A, 456V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4822,"TEM",1,"MC",106,1]
["1PH81331SG000MA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 20KW, 96NM, 45A, 350V 2300RPM,22,5KW, 93NM, 44A, 400V 2650RPM, 24KW, 86NM, 41A, 456V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 19 BIT WITHOUT COMMUTATION POSITION (ENCODER IN19DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: HIGH PERFORMANCE VIBRATION SEVERITY GRADE SPECIAL/B SHAFT AND FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8079,"TEM",1,"MC",106,1]
["1PH81331WF032BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 15KW, 96NM, 34A, 342V 1750RPM,17,5KW, 96NM, 34A, 392V 2000RPM, 20KW, 96NM, 34A, 445V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL 1024 S/R) CONNECTION VIA TERMINAL BLOCK (ADDITIONAL TERMINAL BOX) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5774,"TEM",1,"MC",106,1]
["1PH81332EF221BA1","SIMOTICS M COMPACT SYNCHRONOUS MOTOR 1500RPM,23,1KW,147NM, 42A, 371V 1750RPM,26,4KW,144NM, 42A, 415V 2000RPM, 29KW, 139NM, 41A, 449V WATER COOLING DEGREE OF PROTECTION IP65 ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER AM2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",11176,"TEM",1,"MC",120,1]
["1PH81351AF100BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM,18,5KW,118NM, 43A, 330V 1750RPM,21,5KW,117NM, 43A, 383V 2000RPM, 24KW, 115NM, 43A, 434V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",4526,"TEM",1,"MC",125,1]
["1PH81351AF200BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 22KW, 140NM, 51A, 342V 1750RPM, 25,5KW, 139NM, 51A, 39 2000RPM, 29KW, 138NM, 52A, 448V WATER COOLING DEGREE OF PROTECTION IP65 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5478,"TEM",1,"MC",141,1]
["1PH81351AF232BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 22KW, 140NM, 51A, 342V 1750RPM, 25,5KW, 139NM, 51A, 39 2000RPM, 29KW, 138NM, 52A, 448V WATER COOLING DEGREE OF PROTECTION IP65 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",6020,"TEM",1,"MC",141,1]
["1PH81351DF001LA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM,18,5KW,118NM, 43A, 330V 1750RPM,21,5KW,117NM, 43A, 383V 2000RPM, 24KW, 115NM, 43A, 434V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6480,"TEM",1,"MC",125,1]
["1PH81351DF031CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM,18,5KW,118NM, 43A, 330V 1750RPM,21,5KW,117NM, 43A, 383V 2000RPM, 24KW, 115NM, 43A, 434V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6670,"TEM",1,"MC",125,1]
["1PH81351DF132BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM,18,5KW,118NM, 43A, 330V 1750RPM,21,5KW,117NM, 43A, 383V 2000RPM, 24KW, 115NM, 43A, 434V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",6475,"TEM",1,"MC",125,1]
["1PH81351DS000MA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM,24,5KW,117NM, 51A, 372V 5000RPM,18,5KW, 47NM, 52A, 425V 1500RPM,18,5KW,118NM, 51A, 283V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: HIGH PERFORMANCE VIBRATION SEVERITY GRADE SPECIAL/B SHAFT AND FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7153,"TEM",1,"MC",125,1]
["1PH81351HF022CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM,18,5KW,118NM, 43A, 330V 1750RPM,21,5KW,117NM, 43A, 383V 2000RPM, 24KW, 115NM, 43A, 434V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5348,"TEM",1,"MC",125,1]
["1PH81351HF122CC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM,18,5KW,118NM, 43A, 330V 1750RPM,21,5KW,117NM, 43A, 383V 2000RPM, 24KW, 115NM, 43A, 434V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5348,"TEM",1,"MC",125,1]
["1PH81351HF222CC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 22KW, 140NM, 51A, 342V 1750RPM, 25,5KW, 139NM, 51A, 39 2000RPM, 29KW, 138NM, 52A, 448V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",6300,"TEM",1,"MC",141,1]
["1PH81351JF202CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 22KW, 140NM, 51A, 342V 1750RPM, 25,5KW, 139NM, 51A, 39 2000RPM, 29KW, 138NM, 52A, 448V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",6474,"TEM",1,"MC",141,1]
["1PH81351MF021BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM,18,5KW,118NM, 43A, 330V 1750RPM,21,5KW,117NM, 43A, 383V 2000RPM, 24KW, 115NM, 43A, 434V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5478,"TEM",1,"MC",125,1]
["1PH81351TF031LA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM,18,5KW,118NM, 43A, 330V 1750RPM,21,5KW,117NM, 43A, 383V 2000RPM, 24KW, 115NM, 43A, 434V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 512 S/R WITHOUT C AND D TRACK (ENCODER IC2048S/R) TEMPERATURE SENSOR KTY84-130; DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6545,"TEM",1,"MC",125,1]
["1PH81352DF122CA1","SIMOTICS M COMPACT SYNCHRONOUS MOTOR 1500RPM,23,7KW,151NM, 43A, 383V 1750RPM,27,2KW,149NM, 42A, 415V 2000RPM,30,2KW,144NM, 42A, 449V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",12142,"TEM",1,"MC",120,1]
["1PH81352EG122CA1","SIMOTICS M COMPACT SYNCHRONOUS MOTOR 2000RPM,31,4KW,150NM, 59A, 356V 2300RPM,35,6KW,148NM, 59A, 407V 2650RPM,40,2KW,145NM, 58A, 449V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 ABSOLUTE ENCODER ENDAT 2048 S/R (ENCODER AM2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",12359,"TEM",1,"MC",120,1]
["1PH81352MG132BB1","SIMOTICS M COMPACT SYNCHRONOUS MOTOR 2000RPM,31,4KW,150NM, 59A, 356V 2300RPM,35,6KW,148NM, 59A, 407V 2650RPM,40,2KW,145NM, 58A, 449V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",11557,"TEM",1,"MC",120,1]
["1PH81371AD122CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 17KW, 162NM, 43A, 307V 1150RPM,19,5KW,162NM, 43A, 350V 1350RPM, 22KW, 156NM, 42A, 404V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD VIBRATION SEVERITY GRADE S/A; SHAFT A.FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5235,"TEM",1,"MC",141,1]
["1PH81371AF120BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 22KW, 140NM, 56A, 308V 1750RPM, 25KW, 136NM, 56A, 353V 2000RPM, 28KW, 134NM, 55A, 401V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5040,"TEM",1,"MC",141,1]
["1PH81371AF202CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 27KW, 172NM, 67A, 315V 1750RPM,31,5KW,172NM, 67A, 365V 2000RPM, 36KW, 172NM, 67A, 415V WATER COOLING DEGREE OF PROTECTION IP65 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD VIBRATION SEVERITY GRADE S/A; SHAFT A.FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6204,"TEM",1,"MC",157,1]
["1PH81371AG022BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 28KW, 134NM, 60A, 350V 2300RPM, 29KW,120NM, 56A, 400V 2650RPM, 30KW, 108NM, 52A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5040,"TEM",1,"MC",141,1]
["1PH81371DD020BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 17KW, 162NM, 43A, 307V 1150RPM,19,5KW,162NM, 43A, 350V 1350RPM, 22KW, 156NM, 42A, 404V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6448,"TEM",1,"MC",141,1]
["1PH81371DD030CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 17KW, 162NM, 43A, 307V 1150RPM,19,5KW,162NM, 43A, 350V 1350RPM, 22KW, 156NM, 42A, 404V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",6946,"TEM",1,"MC",141,1]
["1PH81371DD131BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 17KW, 162NM, 43A, 307V 1150RPM,19,5KW,162NM, 43A, 350V 1350RPM, 22KW, 156NM, 42A, 404V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",6751,"TEM",1,"MC",141,1]
["1PH81371DF020GA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 22KW, 140NM, 56A, 308V 1750RPM, 25KW, 136NM, 56A, 352V 2000RPM, 28KW, 134NM, 55A, 401V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD, VIBRATION SEVERITY GRADE: R/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6163,"TEM",1,"MC",141,1]
["1PH81371DF032BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 22KW, 140NM, 56A, 308V 1750RPM, 25KW, 136NM, 56A, 352V 2000RPM, 28KW, 134NM, 55A, 401V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6751,"TEM",1,"MC",141,1]
["1PH81371DF230BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 27KW, 172NM, 67A, 315V 1750RPM,31,5KW,172NM, 67A, 365V 2000RPM, 36KW, 172NM, 67A, 415V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7958,"TEM",1,"MC",157,1]
["1PH81371DG132BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 28KW, 134NM, 60A, 350V 2300RPM, 29KW, 120NM, 56A, 400V 2650RPM, 30KW, 108NM, 52A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",6751,"TEM",1,"MC",141,1]
["1PH81371FD121BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 17KW, 162NM, 43A, 307V 1150RPM,19,5KW,162NM, 43A, 350V 1350RPM, 22KW, 156NM, 42A, 404V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",7358,"TEM",1,"MC",141,1]
["1PH81371HD032BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 17KW, 162NM, 43A, 307V 1150RPM,19,5KW,162NM, 43A, 350V 1350RPM, 22KW, 156NM, 42A, 404V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5733,"TEM",1,"MC",141,1]
["1PH81371HD130CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 17KW, 162NM, 43A, 307V 1150RPM,19,5KW,162NM, 43A, 350V 1350RPM, 22KW, 156NM, 42A, 404V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5928,"TEM",1,"MC",141,1]
["1PH81371HF102CC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 22KW, 140NM, 56A, 308V 1750RPM, 25KW, 136NM, 56A, 353V 2000RPM, 28KW, 134NM, 55A, 401V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5386,"TEM",1,"MC",141,1]
["1PH81371HF200CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 27KW, 172NM, 67A, 315V 1750RPM,31,5KW,172NM, 67A, 365V 2000RPM, 36KW, 172NM, 67A, 415V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",6593,"TEM",1,"MC",157,1]
["1PH81371HG000BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 28KW, 134NM, 60A, 350V 2300RPM, 29KW,120NM, 56A, 400V 2650RPM, 30KW, 108NM, 52A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5191,"TEM",1,"MC",141,1]
["1PH81371JD102BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 17KW, 162NM, 43A, 307V 1150RPM,19,5KW,162NM, 43A, 350V 1350RPM, 22KW, 156NM, 42A, 404V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",5603,"TEM",1,"MC",141,1]
["1PH81371JF001QA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 22KW, 140NM, 56A, 308V 1750RPM, 25KW, 136NM, 56A, 352V 2000RPM, 28KW, 134NM, 55A, 401V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING INCREMENTAL ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5917,"TEM",1,"MC",141,1]
["1PH81371JF131BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 22KW, 140NM, 56A, 308V 1750RPM, 25KW, 136NM, 56A, 353V 2000RPM, 28KW, 134NM, 55A, 401V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",6144,"TEM",1,"MC",141,1]
["1PH81371JF230CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 27KW, 172NM, 67A, 315V 1750RPM,31,5KW,172NM, 67A, 365V 2000RPM, 36KW, 172NM, 67A, 415V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7546,"TEM",1,"MC",157,1]
["1PH81371MD031CC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 17KW, 162NM, 43A, 307V 1150RPM,19,5KW,162NM, 43A, 350V 1350RPM, 22KW, 156NM, 42A, 404V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: S/A, SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",6253,"TEM",1,"MC",141,1]
["1PH81371MG000BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 28KW, 134NM, 60A, 350V 2300RPM, 29KW,120NM, 56A, 400V 2650RPM, 30KW, 108NM, 52A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",5516,"TEM",1,"MC",141,1]
["1PH81371SG031LA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 28KW, 134NM, 60A, 350V 2300RPM, 29KW,120NM, 56A, 400V 2650RPM, 30KW, 108NM, 52A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 19 BIT WITHOUT COMMUTATION POSITION (ENCODER IN19DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE: SPECIAL/B, SHAFT AND FLANGE ACCURACY: SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8642,"TEM",1,"MC",141,1]
["1PH81372DL002BB1","SIMOTICS M COMPACT SYNCHRONOUS MOTOR 2500RPM,48,4KW,185NM, 83A, 371V 2800RPM,53,4KW,182NM, 82A, 415V 3000RPM,56,9KW,181NM, 81A, 449V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",12748,"TEM",1,"MC",136,1]
["1PH81372DL021BA1","SIMOTICS M COMPACT SYNCHRONOUS MOTOR 2500RPM,48,4KW,185NM, 83A, 371V 2800RPM,53,4KW,182NM, 82A, 415V 3000RPM,56,9KW,181NM, 81A, 449V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",12987,"TEM",1,"MC",136,1]
["1PH81372FM021BC1","SIMOTICS M COMPACT SYNCHRONOUS MOTOR 3000RPM,57,5KW,183NM, 104A,370V 3300RPM,62,2KW,180NM, 102A,405V 3600RPM,66,7KW,177NM, 100A,440V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",13897,"TEM",1,"MC",136,1]
["1PH81381AF222BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 30KW, 191NM, 80A, 289V 1750RPM, 33KW, 180NM, 77A, 332V 2000RPM, 37KW, 177NM, 76A, 380V WATER COOLING DEGREE OF PROTECTION IP65 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",6572,"TEM",1,"MC",160,1]
["1PH81381DF230BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 30KW, 191NM, 80A, 289V 1750RPM, 33KW, 180NM, 77A, 332V 2000RPM, 37KW, 177NM, 76A, 380V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",8283,"TEM",1,"MC",160,1]
["1PH81381HF230BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 30KW, 191NM, 80A, 289V 1750RPM, 33KW, 180NM, 77A, 332V 2000RPM, 37KW, 177NM, 76A, 380V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",7265,"TEM",1,"MC",160,1]
["1PH81381JF230BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 30KW, 191NM, 80A, 289V 1750RPM, 33KW, 180NM, 77A, 332V 2000RPM, 37KW, 177NM, 76A, 380V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) with TEMPERAT. SENSOR KTY84-130 DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE: R/A, FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",7677,"TEM",1,"MC",160,1]
["1PH81382DG222QB1","SIMOTICS M COMPACT SYNCHRONOUS MOTOR 2000RPM,59,3KW,283NM,131A, 374V 2300RPM,67,7KW,281NM,130A, 415V 2650RPM,76,3KW,275NM, 30A, 449V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: ADVANCED LIFETIME VIBRATION SEVERITY S/A SHAFT A. FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",13831,"TEM",1,"MC",156,1]
["1PH81631AB120BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 400RPM, 9,5KW, 227NM, 30A, 260V 500RPM, 12KW, 229NM, 30A, 325V 600RPM, 14,5KW,231NM, 30A, 370V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6392,"TEM",1,"MC",196,1]
["1PH81631AD102DA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 22KW, 210NM, 55A, 300V 1150RPM, 25KW, 208NM, 55A, 343V 1350RPM, 28 KW,198NM,52A, 400V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE SR/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6223,"TEM",1,"MC",196,1]
["1PH81631AF100CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 30KW,191NM, 71A, 319V 1750RPM, 34KW,186NM, 70A, 366V 2000RPM, 37KW,177NM, 68A, 416V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",5937,"TEM",1,"MC",196,1]
["1PH81631AF202BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 37KW, 236NM, 84A, 328V 1750RPM, 43KW, 235NM, 84A, 380V 2000RPM, 49KW, 234NM, 84A, 430V WATER COOLING DEGREE OF PROTECTION IP65 W/O ENCODER DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7353,"TEM",1,"MC",229,1]
["1PH81631AG031BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 36KW, 172NM, 83A, 324V 2300RPM, 38KW, 158NM, 78A, 370V 2650RPM, 40KW, 144NM, 76A, 390V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 W/O ENCODER DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6587,"TEM",1,"MC",196,1]
["1PH81631DD000BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 22KW,210NM, 55A, 300V 1150RPM, 25KW,208NM, 55A, 343V 1350RPM, 28KW, 198NM, 52A, 400V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7149,"TEM",1,"MC",196,1]
["1PH81631DD031DA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 22KW,210NM, 55A, 300V 1150RPM, 25KW,208NM, 55A, 343V 1350RPM, 28KW, 198NM, 52A, 400V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE SR/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8281,"TEM",1,"MC",196,1]
["1PH81631DF001BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 30KW, 191NM, 71A, 319V 1750RPM, 34KW, 186NM, 70A, 366V 2000RPM, 37KW, 177NM, 68A, 416V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",7344,"TEM",1,"MC",196,1]
["1PH81631DF202BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 37KW, 236NM, 84A, 328V 1750RPM, 43KW, 235NM, 84A, 380V 2000RPM, 49KW, 234NM, 84A, 430V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",8760,"TEM",1,"MC",229,1]
["1PH81631DF220BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 37KW, 236NM, 84A, 328V 1750RPM, 43KW, 235NM, 84A, 380V 2000RPM, 49KW, 234NM, 84A, 430V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",9215,"TEM",1,"MC",229,1]
["1PH81631FD121BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 22KW, 210NM, 55A, 300V 1150RPM, 25KW, 208NM, 55A, 343V 1350RPM, 28 KW,198NM,52A, 400V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",8905,"TEM",1,"MC",196,1]
["1PH81631HB120BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 400RPM, 9,5KW, 227NM, 30A, 260V 500RPM, 12KW, 229NM, 30A, 325V 600RPM, 14,5KW,231NM, 30A, 370V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",6781,"TEM",1,"MC",196,1]
["1PH81631HD100BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 22KW, 210NM, 55A, 300V 1150RPM, 25KW, 208NM, 55A, 343V 1350RPM, 28 KW,198NM,52A, 400V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6130,"TEM",1,"MC",196,1]
["1PH81631HD132BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 22KW, 210NM, 55A, 300V 1150RPM, 25KW, 208NM, 55A, 343V 1350RPM, 28 KW,198NM,52A, 400V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6976,"TEM",1,"MC",196,1]
["1PH81631HF102GA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 30KW,191NM, 71A, 319V 1750RPM, 34KW,186NM, 70A, 366V 2000RPM, 37KW,177NM, 68A, 416V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6041,"TEM",1,"MC",196,1]
["1PH81631HF200CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 37KW, 236NM, 84A, 328V 1750RPM, 43KW, 235NM, 84A, 380V 2000RPM, 49KW, 234NM, 84A, 430V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7741,"TEM",1,"MC",229,1]
["1PH81631HG030GC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 36KW, 172NM, 83A, 324V 2300RPM, 38KW, 158NM, 78A, 370V 2650RPM, 40KW, 144NM, 76A, 390V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",6496,"TEM",1,"MC",196,1]
["1PH81631JB122CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 400RPM, 9,5KW, 227NM, 30A, 260V 500RPM, 12KW, 229NM, 30A, 325V 600RPM, 14,5KW,231NM, 30A, 370V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7583,"TEM",1,"MC",196,1]
["1PH81631JD102BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 22KW, 210NM, 55A, 300V 1150RPM, 25KW, 208NM, 55A, 343V 1350RPM, 28 KW,198NM,52A, 400V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6737,"TEM",1,"MC",196,1]
["1PH81631JF120BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 30KW,191NM, 71A, 319V 1750RPM, 34KW,186NM, 70A, 366V 2000RPM, 37KW,177NM, 68A, 416V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",7192,"TEM",1,"MC",196,1]
["1PH81631JF202CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 37KW, 236NM, 84A, 328V 1750RPM, 43KW, 235NM, 84A, 380V 2000RPM, 49KW, 234NM, 84A, 430V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8348,"TEM",1,"MC",229,1]
["1PH81631MD031LA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 22KW,210NM, 55A, 300V 1150RPM, 25KW,208NM, 55A, 343V 1350RPM, 28KW, 198NM, 52A, 400V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: PERFORMANCE, VIBRATION SEVERITY GRADE SPECIAL/B; SHAFT A. FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7959,"TEM",1,"MC",196,1]
["1PH81631MF221BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 37KW, 236NM, 84A, 328V 1750RPM, 43KW, 235NM, 84A, 380V 2000RPM, 49KW, 234NM, 84A, 430V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",8717,"TEM",1,"MC",229,1]
["1PH81633DB020AA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 400RPM, 9,5KW, 227NM, 30A, 260V 500RPM, 12KW, 229NM, 30A, 325V 600RPM, 14,5KW,231NM, 30A, 370V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD VIBRATION SEVERITY GRADE A; SHAFT A.FLANGE ACCURACY GR. N TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7411,"TEM",1,"MC",196,1]
["1PH81651AB130BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 400RPM, 13KW, 310NM, 36A, 300V 500RPM, 16KW, 306NM, 36A, 365V 600RPM, 19KW, 302NM, 35A, 420V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",6944,"TEM",1,"MC",230,1]
["1PH81651AF102CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 37KW, 236NM, 78A, 350V 1750RPM, 41KW, 224NM, 76A, 400V 2000RPM, 45KW, 215NM, 75A, 440V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",6684,"TEM",1,"MC",230,1]
["1PH81651AF200CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 46KW, 293NM,104A, 330V 1750RPM, 53KW, 289NM,104A, 374V 2000RPM, 60KW, 287NM,103A, 426V WATER COOLING DEGREE OF PROTECTION IP65 W/O ENCODER DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",8870,"TEM",1,"MC",264,1]
["1PH81651AG102BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 41KW, 196NM, 88A, 350V 2300RPM, 44KW, 183NM, 85A, 394V 2650RPM, 50KW, 180NM, 85A, 440V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 W/O ENCODER DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6489,"TEM",1,"MC",230,1]
["1PH81651DB022BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 400RPM, 13KW, 310NM, 36A, 300V 500RPM, 16KW, 306NM, 36A, 365V 600RPM, 19KW, 302NM, 35A, 420V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8547,"TEM",1,"MC",230,1]
["1PH81651DD021DC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 28KW, 267NM, 71A, 292V 1150RPM, 31KW, 257NM, 69A, 333V 1350RPM, 34KW, 241NM, 66A, 387V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE SR/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",8834,"TEM",1,"MC",230,1]
["1PH81651DD100DA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 28KW, 267NM, 71A, 292V 1150RPM, 31KW, 257NM, 69A, 333V 1350RPM, 34KW, 241NM, 66A, 387V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE SR/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7988,"TEM",1,"MC",230,1]
["1PH81651DF020CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 37KW, 236NM, 78A, 350V 1750RPM, 41KW, 224NM, 76A, 400V 2000RPM, 45KW, 215NM, 75A, 440V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8547,"TEM",1,"MC",230,1]
["1PH81651DF032BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 37KW, 236NM, 78A, 350V 1750RPM, 41KW, 224NM, 76A, 400V 2000RPM, 45KW, 215NM, 75A, 440V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",8547,"TEM",1,"MC",230,1]
["1PH81651DF200DA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 46KW, 293NM,104A, 330V 1750RPM, 53KW, 289NM,104A, 374V 2000RPM, 60KW, 287NM,103A, 426V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE SR/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",10369,"TEM",1,"MC",264,1]
["1PH81651DG002QA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 41KW, 196NM, 88A, 350V 2300RPM, 44KW, 183NM, 85A, 394V 2650RPM, 50KW, 180NM, 85A, 440V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: ADVANCED LIFETIME VIBRATION SEVERITY S/A SHAFT A. FLANGE ACCURACY GR. R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8422,"TEM",1,"MC",230,1]
["1PH81651DG230MA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 53KW, 253NM,110A, 352V 2300RPM, 60KW, 249NM,107A, 410V 2650RPM, 65KW, 234NM,100A, 460V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: HIGH PERFORMANCE VIBRATION SEVERITY GRADE SPECIAL/B SHAFT AND FLANGE ACCURACY GR. SPECIAL TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",12182,"TEM",1,"MC",264,1]
["1PH81651FF101BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 37KW, 236NM, 78A, 350V 1750RPM, 41KW, 224NM, 76A, 400V 2000RPM, 45KW, 215NM, 75A, 440V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",8807,"TEM",1,"MC",230,1]
["1PH81651HB100CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 400RPM, 13KW, 310NM, 36A, 300V 500RPM, 16KW, 306NM, 36A, 365V 600RPM, 19KW, 302NM, 35A, 420V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) DESIGN IM B3 (IM V5, IM V6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6878,"TEM",1,"MC",230,1]
["1PH81651HD021BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 28KW, 267NM, 71A, 292V 1150RPM, 31KW, 257NM, 69A, 333V 1350RPM, 34KW, 241NM, 66A, 387V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",7528,"TEM",1,"MC",230,1]
["1PH81651HD130CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 28KW, 267NM, 71A, 292V 1150RPM, 31KW, 257NM, 69A, 333V 1350RPM, 34KW, 241NM, 66A, 387V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7528,"TEM",1,"MC",230,1]
["1PH81651HF102CB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 37KW, 236NM, 78A, 350V 1750RPM, 41KW, 224NM, 76A, 400V 2000RPM, 45KW, 215NM, 75A, 440V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",7073,"TEM",1,"MC",230,1]
["1PH81651HG032BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 41KW, 196NM, 88A, 350V 2300RPM, 44KW, 183NM, 85A, 394V 2650RPM, 50KW, 180NM, 85A, 440V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",7528,"TEM",1,"MC",230,1]
["1PH81651HG101GA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 41KW, 196NM, 88A, 350V 2300RPM, 44KW, 183NM, 85A, 394V 2650RPM, 50KW, 180NM, 85A, 440V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",6593,"TEM",1,"MC",230,1]
["1PH81651JD122BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM, 28KW, 267NM, 71A, 292V 1150RPM, 31KW, 257NM, 69A, 333V 1350RPM, 34KW, 241NM, 66A, 387V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) DESIGN IM B5 (IMV 1,IM V3) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",7940,"TEM",1,"MC",230,1]
["1PH81651JF120BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 37KW, 236NM, 78A, 350V 1750RPM, 41KW, 224NM, 76A, 400V 2000RPM, 45KW, 215NM, 75A, 440V FORCED VENTILATION; DIRECTION OF AIR FLOW NDE --> DE; DEGREE OF PROTECTION IP55 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",7745,"TEM",1,"MC",230,1]
["1PH81651JF220CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 46KW, 293NM,104A, 330V 1750RPM, 53KW, 289NM,104A, 374V 2000RPM, 60KW, 287NM,103A, 426V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) DESIGN IM B5 (IMV 1,IM V3) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",10321,"TEM",1,"MC",264,1]
["1PH81651MB031BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 400RPM, 13KW, 310NM, 36A, 300V 500RPM, 16KW, 306NM, 36A, 365V 600RPM, 19KW, 302NM, 35A, 420V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7853,"TEM",1,"MC",230,1]
["1PH81651MF001HA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 37KW, 236NM, 78A, 350V 1750RPM, 41KW, 224NM, 76A, 400V 2000RPM, 45KW, 215NM, 75A, 440V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",7113,"TEM",1,"MC",230,1]
["1PH81651MG031CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 2000RPM, 41KW, 196NM, 88A, 350V 2300RPM, 44KW, 183NM, 85A, 394V 2650RPM, 50KW, 180NM, 85A, 440V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER SIN/COS 1VPP 2048 S/R WITH ND-END AT TERMINAL BOX (ENCODER IC2048S/R) DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8048,"TEM",1,"MC",230,1]
["1PH81652DF032CA1","SIMOTICS M COMPACT SYNCHRONOUS MOTOR 1500RPM, 61KW, 390NM,119A, 340V 1750RPM, 69KW, 375NM,115A, 395V 2000RPM, 74KW, 355NM,110A, 445V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",15919,"TEM",1,"MC",218,1]
["1PH81661AF202BC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 52KW, 331NM,116A, 332V 1750RPM, 61KW, 333NM,116A, 381V 2000RPM, 68KW, 325NM,116A, 426V WATER COOLING DEGREE OF PROTECTION IP65 W/O ENCODER DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",9737,"TEM",1,"MC",269,1]
["1PH81661DF201BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 52KW, 331NM,116A, 332V 1750RPM, 61KW, 333NM,116A, 381V 2000RPM, 68KW, 325NM,116A, 426V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IM V5, IM V6) SHAFT WITH FITTED KEY FULL-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",11144,"TEM",1,"MC",269,1]
["1PH81661FF230BA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 52KW, 331NM,116A, 332V 1750RPM, 61KW, 333NM,116A, 381V 2000RPM, 68KW, 325NM,116A, 426V WATER COOLING DEGREE OF PROTECTION IP65 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",12510,"TEM",1,"MC",269,1]
["1PH81661HF232CC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 52KW, 331NM,116A, 332V 1750RPM, 61KW, 333NM,116A, 381V 2000RPM, 68KW, 325NM,116A, 426V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 1024 S/R (ENCODER HTL1024S/R) DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE S/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",10971,"TEM",1,"MC",269,1]
["1PH81661JF232BB1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 52KW, 331NM,116A, 332V 1750RPM, 61KW, 333NM,116A, 381V 2000RPM, 68KW, 325NM,116A, 426V WATER COOLING DEGREE OF PROTECTION IP65 INCREMENT. ENCODER HTL 2048 S/R (ENCODER HTL2048S/R) DESIGN IM B35 (IM V15, IM V35) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE LEFT SIGNAL CONNECTION D-END",11188,"TEM",1,"MC",269,1]
["1PH81662FF230BC1","SIMOTICS M COMPACT SYNCHRONOUS MOTOR 1500RPM, 74KW, 475NM,148A, 355V 1750RPM, 85KW, 460NM,143A, 410V 2000RPM, 89KW, 425NM,138A, 465V WATER COOLING DEGREE OF PROTECTION IP65 ABSOLUTE ENCODER 22 BIT SINGLETURN AND 12 BIT MULTITURN (ENCODER AM22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 (IM V15, IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD WITH FIXED BEARING, VIBRATION SEVERITY GRADE R/A; SHAFT AND FLANGE ACCURACY: R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION LEFT",17719,"TEM",1,"MC",257,1]
["1PH81841AB002AA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 400 RPM,16,3KW,389NM, 49A, 271V 500 RPM,20,5KW,392NM, 49A, 335V 600 RPM, 25KW, 398NM, 49A, 410V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 W/O ENCODER with TEMPERAT. SENSOR KTY84-130 DESIGN IM B3 (IMB6, IMB7, IMB8, IMV6) SHAFT WITH FITTED KEY HALF-KEY BALANCING BEARING: STANDARD VIBRATION SEVERITY GRADE A; SHAFT A.FLANGE ACCURACY GR.N TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",8338,"TEM",1,"MC",350,1]
["1PH81861DF000DC1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1500RPM, 74KW, 471NM,166A, 330V 1750RPM, 85KW, 464NM,164A, 385V 2000RPM, 94KW, 449NM,160A, 445V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B3 (IMB6, IMB7, IMB8, IMV6) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD VIBRATION SEVERITY GRADE SR/A; SHAFT A.FLANGE ACCURACY GR.R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE ND-END SIGNAL CONNECTION RIGHT",14313,"TEM",1,"MC",422,1]
["1PH82281DD030CA1","SIMOTICS M COMPACT ASYNCHRONOUS MOTOR 1000RPM,113KW,1079NM,235A, 340V 1150RPM,129KW,1071NM,235A, 390V 1350RPM,147KW,1040NM,225A, 460V FORCED VENTILATION; DIRECTION OF AIR FLOW DE --> NDE; DEGREE OF PROTECTION IP55 INCREMENTAL ENCODER 22 BIT WITH COMMUTATING POSITION (ENCODER IC22DQ) WITH DRIVE-CLIQ INTERFACE DESIGN IM B35 WITH FLANGE A550 (IM V35) PLAIN SHAFT WITHOUT FITTED KEY; BEARING: STANDARD VIBRATION SEVERITY GRADE S/A SHAFT A.FLANGE ACCURACY GR.R TERMINAL BOX (ABOVE) CABLE ENTRY ON THE RIGHT SIGNAL CONNECTION D-END",28613,"TEM",1,"MC",870,1]
["6AU14102AA000AA0","SIMOTION Drive-based Control Unit D410-2 DP; programmable single-axis motion controller with multi-axis option; interfaces: 5 DI, 8 DI/DO, 3 F-DI, 1 F-DO, 1 AI, 1 encoder, 1 DRIVE-CLiQ, 2 PROFIBUS, 1 ethernet",1964,"TEM",1,"MC",1,1]
["6AU18100BA411XA0","SIMOTION ENGINEERING SYSTEM SCOUT V4.1 SP1 FULL LICENSE CDs INCL. STARTER, RUNTIME, TECHN., DRIVEES BASIC, DOCUMENTATION, UTILITIES FOR FREE",3908,"TEM",1,"MC",0.01,0]
["6AU18100FA220XA0","SIMOTION ENGINEERING SYSTEM SCOUT EXTENSIONS V2.2 CAMTOOL Floating License WITH DATA CARRIER MULTILINGUAL (GER/ENG)",3350,"TEM",1,"MC",0.01,0]
["6AU18101CA412XE0","SIMOTION ENGINEERING SYSTEM SCOUT STANDALONE V4.1 SP2 UPGRADE, Data Carrier DVD INCL. STARTER, RUNTIME, TECHN., DRIVEES BASIC, Documentation, UTILITIES FOR FREE",615,"TEM",1,"MC",0.01,0]
["6AU18101KX300AA8","SIMOTION ENGINEERING SYSTEM DCB STUDIO SOURCE CODE V3.0 (CONTAINED OPEN-SOURCE-SOFTWARE FREE OF CHARGE) DELIVERY ON DATA CARRIER DVD",110,"TEM",1,"MC",0.01,1]
["6AU18208BD200AB0","SIMOTION IT Virtual Machine COMPREHENSIVE IT FUNCTIONS WITH JAVA VIRTUAL MACHINE: RUNTIME ENVIRONMENTAL FOR JAVA- APPLICATIONS ON SIMOTION SINGLE LICENSE FOR ONE DEVICE CONTAIN THE FOLLOWING LICENSES SIMOTION IT DIAG: MLFB: 6AU1820-8BA20-0AB0 SIMOTION IT OPC XML-DA: MLFB: 6AU1820-8BB20-0AB0",1050,"TEM",1,"MC",0.01,0]
["6FX20012DB02","INCREM. ENCODER 6FX2001-2DB02 WITH RS 422 (TTL), 1024 P/R, SYNCHRO-FLANGE SHAFT 6MM OPERATING VOLTAGE: 10 - 30 V UNIVERSAL CABLE OUTLET AXIAL / RADIAL CABLE 1M WITH CONNECTOR",362,"TEM",1,"MC",0.495,1]
["6FX20012HB00","INCREM. ENCODER 6FX2001-2HB00 WITH RS 422 (TTL), 1000 P/R SYNCHRO-FLANGE SHAFT 6MM OPERATING VOLTAGE: 10-30 V AXIAL FLANGE CONNECTOR",362,"TEM",1,"MC",0.25,1]
["6FX20012RA50","INCREM. ENCODER 6FX2001-2RA50 WITH RS 422 (TTL), 500 P/R, CLAMP FLANGE WELLE 10 MM OPERATING VOLTAGE 5 V AXIAL FLANGE CONNECTOR",362,"TEM",1,"MC",0.25,1]
["6FX20012SB50","INCREM. ENCODER 6FX2001-2SB50 WITH RS 422 (TTL), 1500 P/R, CLAMP FLANGE WELLE 10 MM OPERATING VOLTAGE 10 - 30 V AXIAL FLANGE CONNECTOR",362,"TEM",1,"MC",0.25,1]
["6FX20015FD130AA1","ABSOLUTE ENCODER SINGLETURN 6FX2001-5FD13 22 BIT WITH DRIVE-CLIQ; SYNCHR. FLANGE; SHAFT 6MM",1084,"TEM",1,"MC",0.7,1]
["6FX20015SS12","ABSOLUTE VALUE ENCODER 6FX2001-5SS12 SINGLETURN 13 BIT WITH SSI, OPERAT. VOLT. 10-30 V STRIP FLANGE SHAFT 10MM AXIAL FLANGE SOCKET",582,"TEM",1,"MC",0.4,1]
["6FX20021DC001AD0","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX2002-1DC00 (SINAMICS DRIVE CLIQ) CONNECTOR IP20/IP20, WITHOUT 24 V LENGTH (M) = 0 + 0 + 3 + 0",118,"TEM",1,"MC",0.28599999999999998,1]
["6FX20021DC001BE0","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX2002-1DC00 (SINAMICS DRIVE CLIQ) CONNECTOR IP20/IP20, WITHOUT 24 V LENGTH (M) = 0 + 10 + 4 + 0",194,"TEM",1,"MC",1.034,1]
["6FX20030AA50","SIGNAL CONN.,  SUB-D TYPE: 6FX2003-0AA50 50-WAY SOCKET, SCREW-TYPE LOCKING, CABLE CLAMPING  5.5 - 12 MM, PACK = 3 UNITS",144,"ΠΑΚ",1,"MC",0.2,1]
["6FX20030SA30","SIGNAL CONNECTOR 12  PINS TYPE: 6FX2003-0SA30 EXTERNAL THREAD PIN 1 12 POLE INSULATOR 12 PIN CONTACTS (0.08-0.22MM2) 12 PIN CONTACTS (0.20-0.56MM2) 2 CABLE CLAMPINGS 6.5 TILL 10 AND 10.1 TILL 13 MM PACK=1 UNIT",53.7,"TEM",1,"MC",0.104,1]
["6FX20037EX00","MANTLE CLAMP FOR SHIELD TYPE: 6FX2003-7EX00 CONNECTION TO UNIT HOUSING 1 PACK = 25 PIECES (COMPLETE CLAMP WITH SCREW AND LENS)",170,"ΠΑΚ",1,"MC",0.14000000000000001,1]
["6FX20424EA021DF0","PREASSEMBLED SIGNAL CABLE TYPE: 6FX2042-4EA02 MPI BUS CABLE BASE: 6FX2002-4EA02-.... CONNECTOR INCLUDED, MOTOR SIDE LENGTH (M) = 35",1143,"TEM",1,"MC",4.05,1]
["6FX30022CT201AF0","SIGNAL CABLE PREASSEMBLED 6FX3002-2CT20-1AF0 FOR INCR. ENCODER IN S-1FL6 LI 3X2X0.20+2X2X0.25 C MOTION-CONNECT 300 UL/CSA DMAX=7.5MM LENGTH(M) = 5M",87.8,"TEM",1,"MC",0.39200000000000002,1]
["6FX50022AH001AC0","SIGNAL CABLE, PREFABRICATED (HTL IN THE MOTOR 1PH.) 4X2X0.34 + 4X0.5 C UL/CSA, DESINA MOTION-CONNECT 500 DMAX = 9.3 MM, TYPE: 6FX5002-2AH00 LENGTH (M) = 0 + 0 + 2 + 0",85.3,"TEM",1,"MC",0.7,1]
["6FX50022AH001KF0","SIGNAL CABLE, PREFABRICATED (HTL IN THE MOTOR 1PH.) 4X2X0.34 + 4X0.5 C UL/CSA, DESINA MOTION-CONNECT 500 DMAX = 9.3 MM, TYPE: 6FX5002-2AH00 LENGTH (M) = 0 + 90 + 5 + 0",613,"TEM",1,"MC",11.86,1]
["6FX50022CA121EA0","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX5002-2CA12 (HTL AND TTL ENCODER ) 4X2X0.34 + 4X0.5 C, WITHOUT D-SUB CONNECTOR, UL/CSA, DESINA MOTION-CONNECT 500 DMAX = 9.3 MM, LENGTH (M) = 0 + 40 + 0 + 0",312,"TEM",1,"MC",4.91,1]
["6FX50022CA311BA0","SIGNAL CABLE, PREASSEMBLED, (VOLTAGE SIGNAL ENCODER) 3X2X0.14+4X0.14+2X0.5+4X0.23 C UL/CSA, DESINA MOTION CONNECT 500 DMAX = 9.9 MM, TYPE: 6FX5002-2CA31 LENGTH (M) = 0 + 10 + 0 + 0",183,"TEM",1,"MC",1.611,1]
["6FX50022CA311GF0","SIGNAL CABLE, PREASSEMBLED, (VOLTAGE SIGNAL ENCODER) 3X2X0.14+4X0.14+2X0.5+4X0.23 C UL/CSA, DESINA MOTION CONNECT 500 DMAX = 9.9 MM, TYPE: 6FX5002-2CA31 LENGTH (M) = 0 + 60 + 5 + 0",585,"TEM",1,"MC",9.2460000000000004,1]
["6FX50022CC121CF0","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX5002-2CC12 (SSI ASBSOLUTE ENCODER 6FX2001-5) 4X2X0.34 + 4X0.5 C, WITHOUT D-SUB CONNECTOR, UL/CSA, DESINA MOTION-CONNECT 500 DMAX = 9.3 MM, LENGTH (M) = 0 + 20 + 5 + 0",233,"TEM",1,"MC",3.46,1]
["6FX50022CF021AJ0","SIGNAL CABLE, PREASSEMBLED ( RESOLVER IN THE MOTOR ) 3X2X0.14 + 4X0.14 + 2X0.5 C UL/CSA, DESINA, MOTION CONNECT 500, DMAX = 9.3 MM, LENGTH (M)= TYPE: 6FX5002-2CF02 LENGTH (M) = 0 + 0 + 8 + 0",166,"TEM",1,"MC",1.0569999999999999,1]
["6FX50022CF021FA0","SIGNAL CABLE, PREASSEMBLED ( RESOLVER IN THE MOTOR ) 3X2X0.14 + 4X0.14 + 2X0.5 C UL/CSA, DESINA, MOTION CONNECT 500, DMAX = 9.3 MM, LENGTH (M)= TYPE: 6FX5002-2CF02 LENGTH (M) = 0 + 50 + 0 + 0",422,"TEM",1,"MC",5.2990000000000004,1]
["6FX50022CH001AC0","SIGNAL CABLE, PREASSEMBLED (810D/611D TO ENDAT ENCODER) 3X2X0.14+4X0.14+2X0.5 C UL/CSA, DESINA, MOTION CONNECT 500, DMAX = 9.3 MM, TYPE: 6FX5002-2CH00 LENGTH (M) = 0 + 0 + 2 + 0",132,"TEM",1,"MC",0.40100000000000002,1]
["6FX50022CH001DF0","SIGNAL CABLE, PREASSEMBLED (810D/611D TO ENDAT ENCODER) 3X2X0.14+4X0.14+2X0.5 C UL/CSA, DESINA, MOTION CONNECT 500, DMAX = 9.3 MM, TYPE: 6FX5002-2CH00 LENGTH (M) = 0 + 30 + 5 + 0",334,"TEM",1,"MC",3.734,1]
["6FX50022DC001AB5","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX5002-2DC00 (SINAMICS DRIVE CLIQ) CONNECTOR IP20/IP20, WITH 24 V MOTION-CONNECT 500 LENGTH (M) = 0 + 0 + 1 + 0,5",101,"TEM",1,"MC",0.14399999999999999,1]
["6FX50022DC101AJ5","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX5002-2DC10 (SINAMICS DRIVE CLIQ) CONNECTOR IP20/IP67, WITH 24 V MOTION-CONNECT 500 LENGTH (M) = 0 + 0 + 8 + 0,5",163,"TEM",1,"MC",0.72599999999999998,1]
["6FX50022DC101CA0","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX5002-2DC10 (SINAMICS DRIVE CLIQ) CONNECTOR IP20/IP67, WITH 24 V MOTION-CONNECT 500 LENGTH (M) = 0 + 20 + 0 + 0",236,"TEM",1,"MC",1.657,1]
["6FX50022DC101EG0","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX5002-2DC10 (SINAMICS DRIVE CLIQ) CONNECTOR IP20/IP67, WITH 24 V MOTION-CONNECT 500 LENGTH (M) = 0 + 40 + 6 + 0",406,"TEM",1,"MC",3.7629999999999999,1]
["6FX50022DC201AC3","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX5002-2DC20 (SINAMICS DRIVE CLIQ) CONNECTOR IP67/IP67, WITH 24 V MOTION-CONNECT 500 LENGTH (M) = 0 + 0 + 2 + 0,3",140,"TEM",1,"MC",0.23799999999999999,1]
["6FX50022DC201CJ0","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX5002-2DC20 (SINAMICS DRIVE CLIQ) CONNECTOR IP67/IP67, WITH 24 V MOTION-CONNECT 500 LENGTH (M) = 0 + 20 + 8 + 0",304,"TEM",1,"MC",2.3199999999999998,1]
["6FX50022DC301BK0","DRIVE-CLIQ CABLE TYPE: 6FX5002-2DC30 PREASSEMBLED FOR DIRECT MEASURING SYSTEM WITH 24 V CONNECTOR RJ45, IP20 AND MATING PLUG M12, IP67 MOTION CONNECT 500 UL/CSA, DESINA DMAX = 7.1 MM LENGTH (M)= 19",240,"TEM",1,"MC",1.857,1]
["6FX50022DC461BC0","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX5002-2DC46 DRIVE-CLIQ WITH 24 V M12 FEMALE/ M17 MALE SPEED-CONNECT-READY MOTION-CONNECT 500 DMAX=7,1 MM LENGTH (M) = 12",243,"TEM",1,"MC",1.2629999999999999,1]
["6FX50022EQ101DB0","SIGNAL CABLE, PREASSEMBLED (ABSOLUTE ENCODER IN MOTOR) 3X2X0.14+4X0.14+2X0.5+4X0.23 C UL/CSA, DESINA, MOTION CONNECT 500, DMAX = 9.9 MM, TYPE: 6FX5002-2EQ10 LENGTH (M) = 0 + 30 + 1 + 0",326,"TEM",1,"MC",4.42,1]
["6FX50022EQ101JA0","SIGNAL CABLE, PREASSEMBLED (ABSOLUTE ENCODER IN MOTOR) 3X2X0.14+4X0.14+2X0.5+4X0.23 C UL/CSA, DESINA, MOTION CONNECT 500, DMAX = 9.9 MM, TYPE: 6FX5002-2EQ10 LENGTH (M) = 0 + 80 + 0 + 0",672,"TEM",1,"MC",11.231,1]
["6FX50022YA041BA0","CABLE ABSOLUTE ENCODER TYPE: 6FX5002-2YA04 M=010",188,"TEM",1,"MC",1.25,1]
["6FX50025CA381CA0","POWER CABLE, PREASSEMBLED,EXT. 4X2.5 C, CONNECTOR SIZE 1.5 (1FT/1FK TO 611/810D/SIMOVERT) UL/CSA, DESINA, MOTION CONNECT 500, DMAX = 12.9 MM, TYPE: 6FX5002-5CA38 LENGTH (M) = 0 + 20 + 0 + 0",478,"TEM",1,"MC",4.79,1]
["6FX50025CG011BE0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5CG01 4X1.5 C, CONNECTOR SIZE 1 (SINAMICS AC DRIVE) UL/CSA, DESINA, MOTION CONNECT 500, DMAX = 8.4 MM, 0 + 10 + 4 + 0",177,"TEM",1,"MC",1.9530000000000001,1]
["6FX50025CG011GB0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5CG01 4X1.5 C, CONNECTOR SIZE 1 (SINAMICS AC DRIVE) UL/CSA, DESINA, MOTION CONNECT 500, DMAX = 8.4 MM, 0 + 60 + 1 + 0",376,"TEM",1,"MC",7.64,1]
["6FX50025CG121AF0","POWER CABLE PREASSEMBLED 4X2.5 C SPEED CONNECT CONNECTOR GR. 1 FOR SINAMICS POWER MODULE MOTION CONNECT 500 UL/CSA, DESINA DMAX = 10 MM, TYPE: 6FX5002-5CG12 LENGTH (M) = 0 + 0 + 5 + 0",147,"TEM",1,"MC",1.25,1]
["6FX50025CG321AD0","POWER CABLE PREASSEMBLED 4X2.5 C SPEED CONNECT CONNECTOR GR.1.5 (SINAMICS AC DRIVE) UL/CSA, DESINA MOTION CONNECT 500 DMAX = 10 MM, TYPE: 6FX5002-5CG32 LENGTH (M) = + 0 + 0 + 3 + 0",204,"TEM",1,"MC",1,1]
["6FX50025CN011DA0","POWER CABLE PREASSEMBLED 4X1.5 C SPEED CONNECT CONNECTOR GR. 1 (SINAMICS MOTOR MODULE) UL/CSA, DESINA MOTION CONNECT 500 DMAX = 11,5 MM TYPE: 6FX5002-5CN01 LENGTH (M) = + 0 + 30 + 0 + 0",373,"TEM",1,"MC",3.9260000000000002,1]
["6FX50025CN011EA0","POWER CABLE PREASSEMBLED 4X1.5 C SPEED CONNECT CONNECTOR GR. 1 (SINAMICS MOTOR MODULE) UL/CSA, DESINA MOTION CONNECT 500 DMAX = 11,5 MM TYPE: 6FX5002-5CN01 LENGTH (M) = + 0 + 40 + 0 + 0",420,"TEM",1,"MC",5.1360000000000001,1]
["6FX50025CN511BF0","POWER CABLE PREASSEMBLED 4X6 C SPEED CONNECT CONNECTOR GR. 1,5 (SINAMICS MOTOR MODULE) UL/CSA, DESINA MOTION CONNECT 500 DMAX = 15,9 MM TYPE: 6FX5002-5CN51 LENGTH (M) = + 0 + 10 + 5 + 0",474,"TEM",1,"MC",6.0510000000000002,1]
["6FX50025CS011CE0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5CS01 (1FT/1FK/1PH TO SINAMICS) 4X1.5 C, CONNECTOR SIZE 1/1.5 MM2 UL/CSA DESINA, MOTION-CONNECT 500 DMAX = 8.4 MM, LENGTH (M) = 0 + 20 + 4 + 0",345,"TEM",1,"MC",3.2,1]
["6FX50025CS021BA0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5CS02 (1FT/1FK/1PH TO SINAMICS) 4X1.5 C, CONNECTOR OPEN/1.5 MM2 UL/CSA DESINA, MOTION-CONNECT 500 DMAX = 11.5 MM, LENGTH (M) = 0 + 10 + 0 + 0",224,"TEM",1,"MC",1.3919999999999999,1]
["6FX50025CS111GF0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5CS11 (1FT/1FK/1PH TO SINAMICS) 4X2.5 C, CONNECTOR SIZE 1/2.5 MM2 UL/CSA DESINA, MOTION-CONNECT 500 DMAX = 12.9 MM, LENGTH (M) = 0 + 60 + 5 + 0",636,"TEM",1,"MC",13.914,1]
["6FX50025CS141CF0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5CS14 (1FT/1FK/1PH TO SINAMICS) 4X10 C, CONNECTOR SIZE 3 RING CABLE LUG, UL/CSA, DESINA, MOTION-CONNECT 500, DMAX = 20 MM, LENGTH (M) = 0 + 20 + 5 + 0",899,"TEM",1,"MC",18.324999999999999,1]
["6FX50025CS231DD0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5CS23 (1FT/1FK TO SINAMICS) 4X16 C, CONNECTOR SIZE 3/RING CABLE LUG UL/CSA DESINA, MOTION-CONNECT 500 DMAX = 24.2 MM, LENGTH (M) = 0 + 30 + 3 + 0",1496,"TEM",1,"MC",36.082000000000001,1]
["6FX50025CS311GF0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5CS31 (1FT/1FK TO SINAMICS) 4X2.5 C, CONNECTOR SIZE 1.5/2.5 MM2 UL/CSA DESINA, MOTION-CONNECT 500 DMAX = 12.9 MM, LENGTH (M) = 0 + 60 + 5 + 0",700,"TEM",1,"MC",14.106,1]
["6FX50025CS421AG6","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5CS42 (1FT/1FK TO SINAMICS) 4X4 C, MOTORSIDE OPEN END OF CONDUCTORS/4 MM2 UL/CSA DESINA, MOTION-CONNECT 500 DMAX = 14.1 MM, LENGTH (M) = 0 + 0 + 6 + 0,6",244,"TEM",1,"MC",1.9750000000000001,1]
["6FX50025CS521DA0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5CS52 (1FT/1FK TO SINAMICS) 4X6 C, CONNECTOR OPEN/6 MM2 UL/CSA DESINA, MOTION-CONNECT 500 DMAX = 15.9 MM, LENGTH (M) = 0 + 30 + 0 + 0",524,"TEM",1,"MC",11.244,1]
["6FX50025CS611HA0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5CS61 (1FT/1FK TO SINAMICS) 4X10 C, CONNECTOR SIZE 1.5/10 MM2 UL/CSA DESINA, MOTION-CONNECT 500 DMAX = 20.0 MM, LENGTH (M) = 0 + 70 + 0 + 0",1540,"TEM",1,"MC",48.087000000000003,1]
["6FX50025DA201FA0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5DA20 ( 1FK7 AH 20 TO MOTOR MODULE ) 4X1,5+(2X1,5) C; CONNECTOR SIZE 0,5/1,5 SQMM UL/CSA DESINA, MOTION-CONNECT 500 DMAX=13,1 MM, LENGTH (M) = 0 + 50 + 0 + 0",654,"TEM",1,"MC",12.07,1]
["6FX50025DG011AB0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5DG01 4X1.5+(2X1.5)C, CONN. SIZE 1 (SINAMICS AC DRIVE) UL/CSA, DESINA MOTION-CONNECT 500 DMAX=10,8 MM, 0 + 0 + 1 + 0",143,"TEM",1,"MC",0.5,1]
["6FX50025DG101EE0","POWER CABLE PREASSEMBLED 4X1.5+(2X1.5) C SPEED CONNECT CONNECTOR GR. 1 (SINAMICS AC DRIVE) UL/CSA, DESINA MOTION CONNECT 500 DMAX = 10,8 MM TYPE: 6FX5002-5DG10 LENGTH (M) = + 0 + 40 + 4 + 0",457,"TEM",1,"MC",9.93,1]
["6FX50025DG231CF0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5DG23 4X16 + (2X1.5) C, CONN. SIZE 3 (SINAMICS AC DRIVE) UL/CSA DESINA MOTION-CONNECT 500 DMAX=25 MM, ENCLOSURE: 4XCABLE LUGS M8, 1XCABLE LUGS M6, 1XSPRING CLAMP LENGTH (M) = 0 + 20 + 5 + 0",1336,"TEM",1,"MC",28.812000000000001,1]
["6FX50025DN051AF0","POWER CABLE PREASSEMBLED EXT. 4X1.5+(2X1.5) C, SPEED CONNECT CONNECTOR GR. 1 (SINAMICS AC DRIVE) UL/CSA, DESINA MOTION CONNECT 500 DMAX = 13.1 MM TYPE: 6FX5002-5DN05 LENGTH (M) = + 0 + 0 + 5 + 0",263,"TEM",1,"MC",1.35,1]
["6FX50025DN051BC0","POWER CABLE PREASSEMBLED EXT. 4X1.5+(2X1.5) C, SPEED CONNECT CONNECTOR GR. 1 (SINAMICS AC DRIVE) UL/CSA, DESINA MOTION CONNECT 500 DMAX = 13.1 MM TYPE: 6FX5002-5DN05 LENGTH (M) = + 0 + 10 + 2 + 0",315,"TEM",1,"MC",2.89,1]
["6FX50025DN641FH0","POWER CABLE PREASSEMBLED 4X10+2X1,5 C SPEED CONNECT CONNECTOR GR. 1,5 RING CABLE LUG (SINAMICS MOTOR MODULE) UL/CSA, DESINA MOTION CONNECT 500 DMAX = 21,7 MM TYPE: 6FX5002-5DN64 LENGTH (M) = + 0 + 50 + 7 + 0",1408,"TEM",1,"MC",41.466999999999999,1]
["6FX50025DS011AG0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5DS01 (1FT/1FK/1PH TO SINAMICS) 4X1.5+(2X1.5) C, CONNECTOR SIZE 1/1.5 MM2 UL/CSA DESINA, MOTION-CONNECT 500 DMAX = 13.1 MM, LENGTH (M) = 0 + 0 + 6 + 0",296,"TEM",1,"MC",1.629,1]
["6FX50025DS011EF0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5DS01 (1FT/1FK/1PH TO SINAMICS) 4X1.5+(2X1.5) C, CONNECTOR SIZE 1/1.5 MM2 UL/CSA DESINA, MOTION-CONNECT 500 DMAX = 13.1 MM, LENGTH (M) = 0 + 40 + 5 + 0",594,"TEM",1,"MC",10.209,1]
["6FX50025DS211AG0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5DS21 (1FT/1FK/1PH TO SINAMICS) 4X1.5+(2X1.5) C, CONNECTOR SIZE 1.5/1.5 MM2 UL/CSA DESINA, MOTION-CONNECT 500 DMAX = 13.1 MM, LENGTH (M) = 0 + 0 + 6 + 0",360,"TEM",1,"MC",1.821,1]
["6FX50025DS311KF0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5DS31 (1FT/1FK/1PH TO SINAMICS) 4X2.5+(2X1.5) C, CONNECTOR SIZE 1.5/2.5 MM2 UL/CSA DESINA, MOTION-CONNECT 500 DMAX = 14.3 MM, LENGTH (M) = 0 + 90 + 5 + 0",1216,"TEM",1,"MC",24.189,1]
["6FX50025DS411KF0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5DS41 (1FT/1FK/1PH TO SINAMICS) 4X4+(2X1.5) C, CONNECTOR SIZE 1.5/4 MM2 UL/CSA DESINA, MOTION-CONNECT 500 DMAX = 15.4 MM, LENGTH (M) = 0 + 90 + 5 + 0",1505,"TEM",1,"MC",33.109000000000002,1]
["6FX50025DS611FF0","POWER CABLE, PREASSEMBLED TYPE: 6FX5002-5DS61 (1FT/1FK/1PH TO SINAMICS) 4X10+(2X1.5) C, CONNECTOR SIZE 1.5/10 MM2 UL/CSA DESINA, MOTION-CONNECT 500 DMAX = 20.6 MM, LENGTH (M) = 0 + 50 + 5 + 0",1466,"TEM",1,"MC",44.728000000000002,1]
["6FX50081BA216AA0","POWER CABLE, SOLD BY THE METER TYPE: 6FX5008-1BA21 4 X 2.5 + 2 X 1.5 C UL/CSA, DESINA MOTION-CONNECT 500 DELIVERY FORM: ON DISPOS. DRUM DMAX=12.4 MM, LENGTH (M)=500",5554,"TEM",1,"MC",139,1]
["6FX50081BA512AA0","POWER CABLE, SOLD BY THE METER TYPE: 6FX5008-1BA51 4 X 10 + 2 X 1.5 C UL/CSA, DESINA MOTION-CONNECT 500 DELIVERY FORM: ON DISPOS. DRUM DMAX=21.7 MM, LENGTH (M)=100",2478,"TEM",1,"MC",75,1]
["6FX50081BB121FA0","POWER CABLE SOLD BY THE METER TYPE: 6FX5008-1BB12 4 X 120 C UL/CSA, DESINA MOTION-CONNECT 500 DMAX=56.0 MM, LENGTH (M)= 0 + 50 + 0 + 0",9724,"TEM",1,"MC",305.5,1]
["6FX50081BB251HF0","POWER CABLE, SOLD BY THE METER TYPE: 6FX5008-1BB25 4 X 25 C UL/CSA, DESINA MOTION-CONNECT 500 DELIV. FORM:UP TO 19 M IN COILS FROM 20 M IN DRUMS DMAX=28.0 MM, LENGTH (M) = 0 + 70 + 5 + 0",2857,"TEM",1,"MC",106.501,1]
["6FX50081BB351BC0","POWER CABLE, SOLD BY THE METER TYPE: 6FX5008-1BB35 4 X 35 C UL/CSA, DESINA MOTION-CONNECT 500 DELIV. FORM:UP TO 14 M IN COILS FROM 15 M IN DRUMS DMAX=31.5 MM, LENGTH (M) = 0 + 10 + 2 + 0",673,"TEM",1,"MC",22.440999999999999,1]
["6FX50081BB411CH0","POWER CABLE, SOLD BY THE METER TYPE: 6FX5008-1BB41 4 X 6.0 C UL/CSA, DESINA MOTION-CONNECT 500 DELIVERY FORM:TIL 69 M IN COILS FROM 70 M DRUM DMAX =13.6 MM, LENGTH (M) = 0 + 20 + 7 + 0",375,"TEM",1,"MC",12.420999999999999,1]
["6FX50081BB501FH0","POWER CABLE, SOLD BY THE METER TYPE: 6FX5008-1BB50 4 X 50 C UL/CSA, DESINA MOTION-CONNECT 500 DELIV. FORM: UP TO 9 M IN COILS FROM 10 M IN DRUMS DMAX=38.0 MM, LENGTH (M) = 0 + 50 + 7 + 0",4200,"TEM",1,"MC",194.941,1]
["6FX50081BB611JH0","POWER CABLE, SOLD BY THE METER TYPE: 6FX5008-1BB61 4 X 16 C UL/CSA, DESINA MOTION-CONNECT 500 DELIVERY FORM:TIL 29 M IN COILS FROM 30 M DRUM DMAX =24.2 MM, LENGTH (M) = 0 + 80 + 7 + 0",2405,"TEM",1,"MC",95.700999999999993,1]
["6FX50122CA311DA0","SIGNAL CABLE, PREASSEMBLED, (VOLTAGE SIGNAL ENCODER) 3X2X0.14+4X0.14+2X0.5+4X0.23 C UL/CSA, DESINA MOTION CONNECT 500 DMAX = 9.9 MM, TYPE: 6FX5012-2CA31 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = 0 + 30 + 0 + 0",330,"TEM",1,"MC",4.391,1]
["6FX50122CF021FD0","SIGNAL CABLE, PREASSEMBLED ( RESOLVER IN THE MOTOR ) 3X2X0.14 + 4X0.14 + 2X0.5 C UL/CSA, DESINA, MOTION CONNECT 500, DMAX = 9.3 MM, LENGTH (M)= TYPE: 6FX5012-2CF02 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = 0 + 50 + 3 + 0",440,"TEM",1,"MC",5.6020000000000003,1]
["6FX50125CN011BG0","POWER CABLE PREASSEMBLED 4X1.5 C SPEED CONNECT CONNECTOR GR. 1 (SINAMICS MOTOR MODULE) UL/CSA, DESINA MOTION CONNECT 500 DMAX = 11,5 MM TYPE: 6FX5012-5CN01 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = + 0 + 10 + 6 + 0",308,"TEM",1,"MC",2.2320000000000002,1]
["6FX50125DS011DA0","POWER CABLE, PREASSEMBLED TYPE: 6FX5012-5DS01 (1FT/1FK/1PH TO SINAMICS) 4X1.5+(2X1.5) C, CONNECTOR SIZE 1/1.5 MM2 UL/CSA DESINA, MOTION-CONNECT 500 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED DMAX = 13.1 MM, LENGTH (M) = 0 + 30 + 0 + 0",479,"TEM",1,"MC",6.9089999999999998,1]
["6FX70025EA051AK0","POWER CABLE, PREASSEMBLED TYPE: 6FX7002-5EA05 EXTENSION, 4X1.5+(4X0.5)C, CONNECTOR SIZE 1, (1FN TO 611) TRAILING TYPE UL/CSA DESINA MOTION CONNECT 700 DMAX = 14 MM, LENGTH (M) = 0 + 0 + 9 + 0",390,"TEM",1,"MC",2.5499999999999998,1]
["6FX70025EA481BA0","POWER CABLE, PREASSEMBLED TYPE: 6FX7002-5EA48 EXTENSION, 4X4+(4X0.5)C, CONNECTOR SIZE 1.5 (1FN TO 611), UL/CSA, DESINA, TRAILING T.,MOTION CONNECT 700 DMAX = 16.6 MM, LENGTH (M)  = 0 + 10 + 0 + 0",599,"TEM",1,"MC",4.5999999999999996,1]
["6FX70025EB181AD5","POWER CABLE, PREASSEMBLED EXT. TYPE: 6FX7002-5EB18 4X2.5+(4X0.5) C, CONN. SIZE 1 (1FN TO 611), UL/CSA, DESINA, TRAILING T.,MOTION CONNECT 700 DMAX = 15.2 MM, LENGTH (M)  = 0 + 0 + 3 + 0,5",296,"TEM",1,"MC",1.45,1]
["6FX70025LM621AA4","POWER CABLE PREASSAMBLED TYPE: 6FX7002-5LM62 4X2.5 C SCREW GLAND M20/ 1FN3 CONNECTOR FULL THREAD SIZE 1 ON THE CONVERTER SIDE FOR SIMODRIVE/ MASTERDRIVES MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=11 MM LENGTH (M) = 0 + 0 + 0 + 0,4",221,"TEM",1,"MC",0.22900000000000001,1]
["6FX70081BC411BF0","POWER CABLE,SOLD BY THE METER, TYPE: 6FX7008-1BC41 4X6 + 4X0.5 C FOR LINEAR MOTORS TRAILING TYPE UL/CSA DESINA MOTION-CONNECT 700 DELIVERY FORM: IN COILS DMAX = 18.3 MM, LENGTH (M)= 0 + 10 + 5 + 0",517,"TEM",1,"MC",7.8010000000000002,1]
["6FX80021AA141AD0","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX8002-1AA14 CUSTOM MADE LENGTH (M) = 0 + 0 + 3 + 0",172,"TEM",1,"MC",0.25800000000000001,1]
["6FX80022AD041CJ0","SIGNAL CABLE, PREASSEMBLED FOR ABSOLUTE ENCODER SSI AND ENDAT DC 5 V, ALSO EXTENSION FOR BASE 6FX8002-2AD00-XXXX 3X(2X0.14)C + 4X0.14 + 2X0.5 C CONNECTOR FULL THREAD M23 MOTION CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DMAX = 9.2 MM TYPE: 6FX8002-2AD04 LENGTH (M) = 0 + 20 + 8 + 0",442,"TEM",1,"MC",3.0139999999999998,1]
["6FX80022AH111BC0","SIGNAL CABLE PREASSAMBLED ( BASIS 6FX8002-2AH00-.... ) WITH  INTEGRATE TEMPERATURE WIRES TRAILING TYPE UL/CSA DESINA MOTION-CONNECT 800, DMAX = 9.3 MM, TYPE: 6FX8002-2AH11 LENGTH (M) = 0 + 10 + 2 + 0",214,"TEM",1,"MC",1.58,1]
["6FX80022BA201CA0","SIGNAL CABLE, PREASSEMBLED PRESSURE SENSOR TO 611 2X(2X0.18) C OPEN CABLE END MOTION CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DMAX = 5.3 MM, LENGTH (M) = TYPE: 6FX8002-2BA20 LENGTH (M) = 0 + 20 + 0 + 0",259,"TEM",1,"MC",0.88800000000000001,1]
["6FX80022CA311AE0","SIGNAL CABLE, PREASSEMBLED, FOR INCR.ENCODER WITH C/D TRACKS IN MOTOR 3X(2X0.14)C + 4X0,14 + 2X0.5 + 4X0.22 C WITH FULL THREAD CONNECTOR M23 MOTION CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 9.8 MM, LENGTH (M) = TYPE: 6FX8002-2CA31 LENGTH (M) = + 0 + 0 + 4 + 0",179,"TEM",1,"MC",0.45100000000000001,1]
["6FX80022CA311BG0","SIGNAL CABLE, PREASSEMBLED, FOR INCR.ENCODER WITH C/D TRACKS IN MOTOR 3X(2X0.14)C + 4X0,14 + 2X0.5 + 4X0.22 C WITH FULL THREAD CONNECTOR M23 MOTION CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 9.8 MM, LENGTH (M) = TYPE: 6FX8002-2CA31 LENGTH (M) = + 0 + 10 + 6 + 0",301,"TEM",1,"MC",1.5309999999999999,1]
["6FX80022CA311EE0","SIGNAL CABLE, PREASSEMBLED, FOR INCR.ENCODER WITH C/D TRACKS IN MOTOR 3X(2X0.14)C + 4X0,14 + 2X0.5 + 4X0.22 C WITH FULL THREAD CONNECTOR M23 MOTION CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 9.8 MM, LENGTH (M) = TYPE: 6FX8002-2CA31 LENGTH (M) = + 0 + 40 + 4 + 0",585,"TEM",1,"MC",4.0510000000000002,1]
["6FX80022CA341GF0","SIGNAL CABLE, EXTENSION FOR BASE -2CA31-2CA80 OR -2CA 88 3X(2X0.14)C + 4X0,14 + 2X0.5  + 4X0.22 C WITH FULL THREAD CONNECTOR M23 MOTION CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DMAX = 9.8 MM LENGTH = TYPE: 6FX8002-2CA34 LENGTH (M) = 0 + 60 + 5 + 0",819,"TEM",1,"MC",9.2159999999999993,1]
["6FX80022CA801EA0","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX8002-2CA80 FOR INCREMENTAL ENCODER SIN/COS 1 VPP WITHOUT TRACK C- AND D 3X(2X0.14)C + 4X0.14 + 2X0.5 C CONNECTOR FULL THREAD M23 MOTION CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DMAX = 9.2 MM LENGTH (M) = 0 + 40 + 0 + 0",549,"TEM",1,"MC",4.4009999999999998,1]
["6FX80022CB541CF0","SIGNAL CABLE EXTENSION FOR BASE 6FX8002-2CA12, -2CR00, -CD24, -2CG00, - 2CC11 4X(2X0.34) + 4X0.5 C CONNECTOR FULL THREAD M23 ANGLED MOTION CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DMAX = 9.3 MM LENGTH (M) = TYPE: 6FX8002-2CB54 LENGTH (M) = 0 + 20 + 5 + 0",305,"TEM",1,"MC",3.1720000000000002,1]
["6FX80022CD011AH0","SIGNAL CABLE, PREASSEMBLED FOR INCR. ENCODER TTL RS422 DC 5V, 6FX2001-2 TO FM357-2 4X(2X0.34) + 4X0.5 C CONNECTOR FULL THREAD M23 MOTION CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 9.3 MM, LENGTH (M) = TYPE: 6FX8002-2CD01 LENGTH (M) = + 0 + 0 + 7 + 0",155,"TEM",1,"MC",1.022,1]
["6FX80022CF021AD0","SIGNAL CABLE, PREASSEMBLED FOR RESOLVER 3X(2X0.14)C + 4X0.14 + 2X0.5 C CONNECTOR FULL THREAD M23 MOTION CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DMAX = 9.2 MM LENGTH (M) = TYPE: 6FX8002-2CF02 LENGTH (M) = 0 + 0 + 3 + 0",165,"TEM",1,"MC",0.438,1]
["6FX80022CF021GA0","SIGNAL CABLE, PREASSEMBLED FOR RESOLVER 3X(2X0.14)C + 4X0.14 + 2X0.5 C CONNECTOR FULL THREAD M23 MOTION CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DMAX = 9.2 MM LENGTH (M) = TYPE: 6FX8002-2CF02 LENGTH (M) = 0 + 60 + 0 + 0",741,"TEM",1,"MC",6.1950000000000003,1]
["6FX80022CG001AD0","SIGNAL CABLE, PREASSEMBLED FOR INCREMENTAL ENCODER SIN/COS 1VPP, 6FX2001-3 4X(2X0.34) + 4X0.5 C CONNECTOR FULL THREAD M23 MOTION CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 9.3 MM LENGTH (M) = TYPE: 6FX8002-2CG00 LENGTH (M) = 0 + 0 + 3 + 0",125,"TEM",1,"MC",0.48199999999999998,1]
["6FX80022CH001AG4","SIGNAL CABLE, PREASSEMBLED, FOR ABSOLUTE ENCODER ENDAT 6FX2001-5 3X(2X0.14)C + 4X0.14 + 2X0.5 C CONNECTOR FULL THREAD M23 MOTION CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 9.2 MM LENGTH (M) = TYPE: 6FX8002-2CH00 LENGTH (M) = 0 + 0 + 6 + 0,4",210,"TEM",1,"MC",0.78200000000000003,1]
["6FX80022CH001DD0","SIGNAL CABLE, PREASSEMBLED, FOR ABSOLUTE ENCODER ENDAT 6FX2001-5 3X(2X0.14)C + 4X0.14 + 2X0.5 C CONNECTOR FULL THREAD M23 MOTION CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 9.2 MM LENGTH (M) = TYPE: 6FX8002-2CH00 LENGTH (M) = 0 + 30 + 3 + 0",472,"TEM",1,"MC",3.4689999999999999,1]
["6FX80022CP001AH0","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX8002-2CP00 FOR HANDWHEEL 840D ON COM BOARD 4X(2X0.18) C MOTION CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DMAX = 6.7 MM LENGTH (M) = 0 + 0 + 7 + 0",123,"TEM",1,"MC",0.53600000000000003,1]
["6FX80022DC001AF0","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX8002-2DC00 (SINAMICS DRIVE CLIQ) CONNECTOR IP20/IP20, WITH 24 V MOTION-CONNECT 800 RELEASED ONLY UP TO 50 M LENGTH (M) = 0 + 0 + 5 + 0",161,"TEM",1,"MC",0.39400000000000002,1]
["6FX80022DC001GA0","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX8002-2DC00 (SINAMICS DRIVE CLIQ) CONNECTOR IP20/IP20, WITH 24 V MOTION-CONNECT 800 RELEASED ONLY UP TO 50 M LENGTH (M) = 0 + 60 + 0 + 0",755,"TEM",1,"MC",4.1340000000000003,1]
["6FX80022DC101AK2","PRE-ASSEMBLED SIGNAL CABLE TYPE: 6FX8002-2DC10 DRIVE-CLIQ WITH 24V RJ45 CONNECTOR; IP20 ON MODULE SIDE AND IP67 ON MOTOR SIDE, MOTION-CONNECT 800PLUS APPROVED ONLY UP TO A LENGTH OF 75M, DMAX=7.1 MM LENGTH (M) = 0 + 0 + 9 + 0,2",199,"TEM",1,"MC",0.65500000000000003,1]
["6FX80022DC101BJ0","PRE-ASSEMBLED SIGNAL CABLE TYPE: 6FX8002-2DC10 DRIVE-CLIQ WITH 24V RJ45 CONNECTOR; IP20 ON MODULE SIDE AND IP67 ON MOTOR SIDE, MOTION-CONNECT 800PLUS APPROVED ONLY UP TO A LENGTH OF 75M, DMAX=7.1 MM LENGTH (M) = 0 + 10 + 8 + 0",262,"TEM",1,"MC",1.2529999999999999,1]
["6FX80022DC101DJ0","PRE-ASSEMBLED SIGNAL CABLE TYPE: 6FX8002-2DC10 DRIVE-CLIQ WITH 24V RJ45 CONNECTOR; IP20 ON MODULE SIDE AND IP67 ON MOTOR SIDE, MOTION-CONNECT 800PLUS APPROVED ONLY UP TO A LENGTH OF 75M, DMAX=7.1 MM LENGTH (M) = 0 + 30 + 8 + 0",418,"TEM",1,"MC",2.613,1]
["6FX80022DC201AE0","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX8002-2DC20 (SINAMICS DRIVE CLIQ) CONNECTOR IP67/IP67, WITH 24 V MOTION-CONNECT 800 LENGTH (M) = 0 + 0 + 4 + 0",170,"TEM",1,"MC",0.314,1]
["6FX80022DC301CJ1","DRIVE-CLIQ CABLE TYPE: 6FX8002-2DC30 PREASSEMBLED FOR DIRECT MEASURING SYSTEM WITH 24 V CONNECTOR RJ45, IP20 AND MATING PLUG M12, IP67 MOTION CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX = 7.1 MM LENGTH (M)= 28,1",373,"TEM",1,"MC",1.835,1]
["6FX80022DC461AH0","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX8002-2DC46 DRIVE-CLIQ WITH 24 V M12 FEMALE/ M17 MALE SPEED-CONNECT-READY MOTION-CONNECT 800PLUS UL/CSA, DESINA,  TRAILING TYPE DMAX=7,1 MM LENGTH (M) = 7",219,"TEM",1,"MC",0.58699999999999997,1]
["6FX80022EQ101AK5","SIGNAL CABLE, PREASSEMBLED, FOR ABSOLUTE ENCODER ENDAT IN MOTOR 3X(2X0.14)C + 4X0,14 + 2X0.5 + 4X0.22 C CONNECTOR FULL THREAD M23 MOTION CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 9.8 MM LENGTH = TYPE: 6FX8002-2EQ10 LENGTH (M) = 0 + 0 + 9 + 0,5",240,"TEM",1,"MC",1.4510000000000001,1]
["6FX80022EQ101CF0","SIGNAL CABLE, PREASSEMBLED, FOR ABSOLUTE ENCODER ENDAT IN MOTOR 3X(2X0.14)C + 4X0,14 + 2X0.5 + 4X0.22 C CONNECTOR FULL THREAD M23 MOTION CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 9.8 MM LENGTH = TYPE: 6FX8002-2EQ10 LENGTH (M) = 0 + 20 + 5 + 0",392,"TEM",1,"MC",3.605,1]
["6FX80022EQ101GB0","SIGNAL CABLE, PREASSEMBLED, FOR ABSOLUTE ENCODER ENDAT IN MOTOR 3X(2X0.14)C + 4X0,14 + 2X0.5 + 4X0.22 C CONNECTOR FULL THREAD M23 MOTION CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 9.8 MM LENGTH = TYPE: 6FX8002-2EQ10 LENGTH (M) = 0 + 60 + 1 + 0",755,"TEM",1,"MC",8.609,1]
["6FX80022EQ141AF5","SIGNAL CABLE, EXTENSION FOR BASE 6FX8002-2EQ10-.... 3X(2X0.14)C + 4X0,14 + 2X0.5 + 4X0.22 C CONNECTOR FULL THREAD M23 MOTION CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 9.8 MM LENGTH = TYPE: 6FX8002-2EQ14 LENGTH (M) = 0 + 0 + 5 + 0,5",222,"TEM",1,"MC",0.94599999999999995,1]
["6FX80022EQ141CB0","SIGNAL CABLE, EXTENSION FOR BASE 6FX8002-2EQ10-.... 3X(2X0.14)C + 4X0,14 + 2X0.5 + 4X0.22 C CONNECTOR FULL THREAD M23 MOTION CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 9.8 MM LENGTH = TYPE: 6FX8002-2EQ14 LENGTH (M) = 0 + 20 + 1 + 0",375,"TEM",1,"MC",3.1,1]
["6FX80022MK001BA0","SIGNAL CABLE, PREASSEMBLED TYPE: 6FX8002-2MK00 MAIN CABLE 6FX8002-2CA31-.... CUSTOMIZED, MOTION-CONNECT 800, LENGTH (M) = 0 +10 +0 +0",253,"TEM",1,"MC",1.04,1]
["6FX80024AA211AF0","SIGNAL CABLE, PREASSEMBLED, 840C/CSB-I/O UNIT 4X(2X0.18) C MOTION CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DMAX = 6.7 MM LENGTH (M) = TYPE: 6FX8002-4AA21 LENGTH (M) = +0 +0 +5 +0",106,"TEM",1,"MC",0.4,1]
["6FX80024AA411AF5","SIGNAL CABLE, PREASSEMBLED, I/O UNITS TO 840D AND 840C 2X(2X0.18) C MOTION CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DMAX = 5.3 MM LENGTH (M) = TYPE: 6FX8002-4AA41 LENGTH (M) = +0 +0 +5 + 0,5",85.699999999999989,"TEM",1,"MC",0.32,1]
["6FX80025CA051BG0","POWER CABLE, EXTENSION 4 X 1.5 C, CONNECTOR FULL THREAD SIZE 1 MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 9.5 MM, LENGTH (M) = TYPE: 6FX8002-5CA05 LENGTH (M) = 0 + 10 + 6 + 0",419,"TEM",1,"MC",2.7050000000000001,1]
["6FX80025CA281BF0","POWER CABLE, EXTENSION 4 X 1.5 C, CONNECTOR FULL THREAD SIZE 1.5 MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 9.5 MM, LENGTH (M) = TYPE: 6FX8002-5CA28 LENGTH (M) = 0 + 10 + 5 + 0",546,"TEM",1,"MC",2.907,1]
["6FX80025CA581AB0","POWER CABLE EXTENSION 4X6 C CONNECTOR FULL THREAD SIZE 1.5 MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=14.9 MM LENGTH (M) = TYPE: 6FX8002-5CA58 LENGTH (M) = 0 + 0 + 1 + 0",402,"TEM",1,"MC",1.0189999999999999,1]
["6FX80025CA681AG5","POWER CABLE EXTENSION 4X10 C CONNECTOR FULL THREAD SIZE 1.5 MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=18.2 MM LENGTH (M) = TYPE: 6FX8002-5CA68 LENGTH (M) = 0 + 0 + 6 + 0,5",626,"TEM",1,"MC",4.734,1]
["6FX80025CG111CF0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5CG11 4X2.5 C CONNECTOR FULL THREAD SIZE 1 FOR SINAMICS S120 POWER MODULE AND MOTOR MODULE BOOKSIZE COMPACT MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=11 MM LENGTH (M) = + 0 + 20 + 5 + 0",467,"TEM",1,"MC",5.1340000000000003,1]
["6FX80025CG121AF0","POWER CABLE PREASSEMBLED 4X2.5 C CONNECTOR SPEED-CONNECT SIZE 1 FOR SINAMICS S120 POWER MODULE AND MOTOR MOD. BOOKSIZE COMPACT MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=11 MM LENGTH (M) = TYPE: 6FX8002-5CG12 LENGTH (M) = 0 + 0 + 5 + 0",193,"TEM",1,"MC",1.61,1]
["6FX80025CN011BF0","POWER CABLE PREASSEMBLED 4X1,5 C, SPEED-CONNECT GR. 1 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=9.5 MM, TYPE: 6FX8002-5CN01 LENGTH (M) = + 0 + 10 + 5 + 0",435,"TEM",1,"MC",2.5819999999999999,1]
["6FX80025CN051BG8","POWER CABLE PREASSEMBLED EXT. 4X1,5 C, SPEED-CONNECT GR. 1 MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=9.5 MM, TYPE: 6FX8002-5CN05 LENGTH (M) = + 0 + 10 + 6 + 0,8",431,"TEM",1,"MC",2.8290000000000002,1]
["6FX80025CN211BH0","POWER CABLE PREASSEMBLED 4X1,5 C, SPEED-CONNECT GR. 1.5 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=9.5 MM, LONGITUD (M) = TYPE: 6FX8002-5CN21 LENGTH (M) = + 0 + 10 + 7 + 0",528,"TEM",1,"MC",3.0840000000000001,1]
["6FX80025CN311CD0","POWER CABLE PREASSEMBLED 4X2.5 C, CONNECTOR SPEED CONNECT CONNECTOR GR.1.5 FOR SINAMICS S120 MOTOR MODULE BOOKSIZE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=11 MM LENGTH (M) = TYPE: 6FX8002-5CN31 LENGTH (M) = + 0 + 20 + 3 + 0",651,"TEM",1,"MC",5.742,1]
["6FX80025CN511BJ0","POWER CABLE PREASSEMBLED 4X6 C, CONNECTOR SPEED-CONNECT SIZE 1.5 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=14.9 MM LENGTH (M) = TYPE: 6FX8002-5CN51 LENGTH (M) = + 0 + 10 + 8 + 0",737,"TEM",1,"MC",7.9740000000000002,1]
["6FX80025CN541FD0","POWER CABLE PREASSEMBLED 4X6 C, CONNECTOR STECKER SPEED-CONNECT GR. 1.5 RING TERMINAL END ON MOD. SIDE FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=14.9 MM LENGTH (M) = TYPE: 6FX8002-5CN54 LENGTH (M) = + 0 + 50 + 3 + 0",1423,"TEM",1,"MC",22.561,1]
["6FX80025CP421AD0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5CP42 4X10 C, SCREW GLAND M40 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800 TRAILING TYPE, UL/CSA DESINA DMAX=19.4 MM, LENGTH (M) = 0 + 0 + 3 + 0",376,"TEM",1,"MC",3.1320000000000001,1]
["6FX80025CR411FA0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5CR41 4X10 C, SCREW GLAND M32 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800 TRAILING TYPE, UL/CSA DESINA DMAX=18,2 MM, LENGTH (M) = 0 + 50 + 0 + 0 + 0",1587,"TEM",1,"MC",32.450000000000003,1]
["6FX80025CS011BA7","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5CS01 4 X 1.5 C, CONNECTOR FULL THREAD SIZE 1 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DMAX = 9.5 MM, LENGTH (M) = 0 + 10 + 0 + 0,7",385,"TEM",1,"MC",1.9159999999999999,1]
["6FX80025CS011DA0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5CS01 4 X 1.5 C, CONNECTOR FULL THREAD SIZE 1 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DMAX = 9.5 MM, LENGTH (M) = 0 + 30 + 0 + 0",622,"TEM",1,"MC",4.907,1]
["6FX80025CS111BF0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5CS11 4X2.5 C CONNECTOR FULL THREAD SIZE 1 FOR SINAMICS S120 MOTOR MODULE BOOKSIZE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=11 MM LENGTH (M) = 0 + 10 + 5 + 0",467,"TEM",1,"MC",3.71,1]
["6FX80025CS141BC0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5CS14 (1FT/1FK TO SINAMICS) 4X10 C, CONNECTOR SIZE 3 RING TERMINAL END UL/CSA DESINA; TRAILING TYPE, MOTION-CONNECT 800, DMAX = 19.4 MM, LENGTH (M)= 0 + 10 + 2 + 0",823,"TEM",1,"MC",9.0670000000000002,1]
["6FX80025CS211EF0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5CS21 4 X 1.5 C, CONNECTOR FULL THREAD SIZE 1.5 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DMAX = 9.5 MM, LENGTH (M) = 0 + 40 + 5 + 0",876,"TEM",1,"MC",7.4240000000000004,1]
["6FX80025CS241BC0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5CS24 4X16 C CONNECTOR FULL THREAD SIZE 1.5 FOR SINAMICS S120 MOTOR MODULE BOOKSIZE MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DMAX=22.3 MM LENGTH (M)= 0 + 10 + 2 + 0",618,"TEM",1,"MC",11.65,1]
["6FX80025CS311FA0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5CS31 4X2.5 C CONNECTOR FULL THREAD SIZE 1.5 FOR SINAMICS S120 MOTOR MODULE BOOKSIZE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=11 MM LENGTH (M) = 0 + 50 + 0 + 0",1041,"TEM",1,"MC",11.952,1]
["6FX80025CS311FK0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5CS31 4X2.5 C CONNECTOR FULL THREAD SIZE 1.5 FOR SINAMICS S120 MOTOR MODULE BOOKSIZE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=11 MM LENGTH (M) = 0 + 50 + 9 + 0",1171,"TEM",1,"MC",14.022,1]
["6FX80025CS511CG0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5CS51 4X6 C CONNECTOR FULL THREAD SIZE 1.5 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DMAX=14.9 MM LENGTH (M) = 0 + 20 + 6 + 0",922,"TEM",1,"MC",11.334,1]
["6FX80025CS611AJ0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5CS61 (1FT/1FK/1PH TO SINAMICS) 4X10 C, CONNECTOR SIZE 1.5/10 MM2 TRAILING TYPE, UL/CSA DESINA MOTION-CONNECT 800, DMAX = 19.4 MM, LENGTH (M)= 0 + 0 + 8 + 0",603,"TEM",1,"MC",5.423,1]
["6FX80025CS641AG0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5CS64 (1FT/1FK/1PH TO SINAMICS) 4X10 C, CONNECTOR SIZE 1.5/RING CABLE LUG, UL/CSA DESINA, TRAILING TYPE MOTION-CONNECT 800, DMAX = 18.4 MM, LENGTH (M) = 0 + 0 + 6 + 0",417,"TEM",1,"MC",4.0609999999999999,1]
["6FX80025CS641CK0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5CS64 (1FT/1FK/1PH TO SINAMICS) 4X10 C, CONNECTOR SIZE 1.5/RING CABLE LUG, UL/CSA DESINA, TRAILING TYPE MOTION-CONNECT 800, DMAX = 18.4 MM, LENGTH (M) = 0 + 20 + 9 + 0",1171,"TEM",1,"MC",18.459,1]
["6FX80025DA051AG2","POWER CABLE, PREASSEMBLED EXT. 4X1.5+(2X1.5)C, CONNECTOR FULL THREAD SIZE 1 MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX= 12 MM, LENGTH (M) = TYPE: 6FX8002-5DA05 LENGTH (M) = 0 + 0 + 6 + 0,2",350,"TEM",1,"MC",1.704,1]
["6FX80025DA151AB0","POWER CABLE EXTENSION 4X2.5 + (2X1.5)C C MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=13.8 MM LENGTH (M) = TYPE: 6FX8002-5DA15 LENGTH (M) = 0 + 0 + 1 + 0",262,"TEM",1,"MC",0.497,1]
["6FX80025DA281AC5","POWER CABLE, PREASSEMBLED EXT. 4X1.5+(2X1.5)C, CONNECTOR FULL THREAD SIZE 1.5 MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX= 12 MM, LENGTH (M) = TYPE: 6FX8002-5DA28 LENGTH (M) = 0 + 0 + 2 + 0,5",425,"TEM",1,"MC",1.149,1]
["6FX80025DA381AG2","POWER CABLE EXTENSION 4X2.5 + (2X1.5)C C CONNECTOR FULL THREAD SIZE 1.5 MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=13.8 MM LENGTH (M) = TYPE: 6FX8002-5DA38 LENGTH (M) = 0 + 0 + 6 + 0,2",508,"TEM",1,"MC",2.4169999999999998,1]
["6FX80025DA481BB5","POWER CABLE EXTENSION 4X4+(2X1.5)C, CONN. SIZE 1.5 CONNECTOR FULL THREAD SIZE 1.5 MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=15.2 MM LENGTH (M) = TYPE: 6FX8002-5DA48 LENGTH (M) = 0 + 10 + 1 + 0,5",642,"TEM",1,"MC",5.1070000000000002,1]
["6FX80025DA681AH0","POWER CABLE EXTENSION 4X10 + (2X1.5)C C, CONNECTOR FULL THREAD SIZE 1.5 FOR SIMODRIVE/MASTERDRIVES MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=20.1 MM LENGTH (M) = TYPE: 6FX8002-5DA68 LENGTH (M) = 0 + 0 + 7 + 0",690,"TEM",1,"MC",5.9130000000000003,1]
["6FX80025DG011BC0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5DG01 4X1,5+(2X1,5)C C, CONNECTOR FULL THREAD SIZE 1 FOR SINAMICS POWER MODULE MOTION-CONNECT 800PLUS DMAX= 12 MM, LENGTH (M) = + 0 + 10 + 2 + 0",330,"TEM",1,"MC",3.028,1]
["6FX80025DG131AF5","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5DG13 4X10 + (2X1.5)C C; CONNECTOR FULL THREAD SIZE 3; FOR SINAMICS S120 POWER MODULE AND MOTOR MODULE BOOKSIZE COMPACT MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA  DMAX=20.1 MM LENGTH (M) = 0 + 0 + 5 + 0,5",913,"TEM",1,"MC",5.2779999999999996,1]
["6FX80025DG331BA0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5DG33 4X25 + (2X1.5)C C CONNECTOR FULL THREAD SIZE 3 CUTTED WIRE END; LENGTH 300 MM, FUER SINAMICS S120 MOTOR MODULE AND POWER MODULE UL/CSA DESINA MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=27.6 MM ENCLOSURE: 4XCABLE LUGS M8, 1XCABLE LUGS M6, 1XSPRING CLAMP 0 + 10 + 0 + 0",1912,"TEM",1,"MC",15.694000000000001,1]
["6FX80025DN011BE0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5DN01 4X1,5 + (2X1.5)C C, CONNECTOR SPEED CONNECT SIZE 1 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX= 12 MM, LENGTH (M) = 0 + 10 + 4 + 0",492,"TEM",1,"MC",3.6459999999999999,1]
["6FX80025DN011CA5","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5DN01 4X1,5 + (2X1.5)C C, CONNECTOR SPEED CONNECT SIZE 1 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX= 12 MM, LENGTH (M) = 0 + 20 + 0 + 0,5",605,"TEM",1,"MC",5.2190000000000003,1]
["6FX80025DN211CF0","POWER CABLE PREASSEMBLED 4X1,5 + (2X1.5)C C, CONNECTOR SPEED CONNECT SIZE 1.5 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX= 12 MM, LENGTH (M) = TYPE: 6FX8002-5DN21 LENGTH (M) = + 0 + 20 +  5 + 0",738,"TEM",1,"MC",6.5,1]
["6FX80025DN411AB2","POWER CABLE PREASSEMBLED 4X4 + (2X1.5)C C, CONNECTOR SPEED-CONNECT SIZE 1.5 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=15.2 MM LENGTH (M) = TYPE: 6FX8002-5DN41 LENGTH (M) = + 0 + 0 + 1 + 0,2",383,"TEM",1,"MC",0.92800000000000005,1]
["6FX80025DN511JB0","POWER CABLE PREASSEMBLED 4X6 + (2X1.5)C C CONNECTOR SPEED-CONNECT SIZE 1.5 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=17.3 MM LENGTH (M) = TYPE: 6FX8002-5DN51 LENGTH (M) = + 0 + 80 + 1 + 0",2645,"TEM",1,"MC",43.078000000000003,1]
["6FX80025DQ281BA0","POWER CABLE PREASSEMBLED EXT. 4X1,5 + (2X1.5)C C, CONNECTOR SPEED CONNECT GR.1.5 MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX= 12 MM, LENGTH (M) = TYPE: 6FX8002-5DQ28 LENGTH (M) = + 0 + 10 + 0 + 0",534,"TEM",1,"MC",2.964,1]
["6FX80025DS011AE0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5DS01 4X1,5 + (2X1.5)C C, CONNECTOR FULL THREAD SIZE 1 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX= 12 MM, LENGTH (M) = 0 + 0 + 4 + 0",330,"TEM",1,"MC",1.226,1]
["6FX80025DS011BK0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5DS01 4X1,5 + (2X1.5)C C, CONNECTOR FULL THREAD SIZE 1 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX= 12 MM, LENGTH (M) = 0 + 10 + 9 + 0",572,"TEM",1,"MC",4.8559999999999999,1]
["6FX80025DS011GA0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5DS01 4X1,5 + (2X1.5)C C, CONNECTOR FULL THREAD SIZE 1 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX= 12 MM, LENGTH (M) = 0 + 60 + 0 + 0",1235,"TEM",1,"MC",14.778,1]
["6FX80025DS111CF0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5DS11 4X2.5 + (2X1.5)C C CONNECTOR FULL THREAD SIZE 1 FOR SINAMICS S120 MOTOR MODULE BOOKSIZE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=13.9 MM LENGTH (M) = 0 + 20 + 5 + 0",735,"TEM",1,"MC",7.8239999999999998,1]
["6FX80025DS131CA0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5DS13 4X10 + (2X1.5)C C CONNECTOR FULL THREAD SIZE 3 FOR SINAMICS S120 MOTOR MODULE BOOKSIZE MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DMAX=20.1 MM LENGTH (M)= 0 + 20 + 0 + 0",1643,"TEM",1,"MC",16.696999999999999,1]
["6FX80025DS211CD0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5DS21 4X1,5 + (2X1.5)C C, CONNECTOR FULL THREAD SIZE 1,5 MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX= 12 MM, LENGTH (M) = 0 + 20 + 3 + 0",705,"TEM",1,"MC",6.016,1]
["6FX80025DS311AK0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5DS31 4X2.5 + (2X1.5)C C, FULL THREAD CONNECTOR SIZE 1.5 FOR SINAMICS S120 MOTOR MODULE BOOKSIZE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=13.9 MM LENGTH (M) = 0 + 0 + 9 + 0",506,"TEM",1,"MC",3.1859999999999999,1]
["6FX80025DS311GF0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5DS31 4X2.5 + (2X1.5)C C, FULL THREAD CONNECTOR SIZE 1.5 FOR SINAMICS S120 MOTOR MODULE BOOKSIZE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=13.9 MM LENGTH (M) = 0 + 60 + 5 + 0",1553,"TEM",1,"MC",20.097999999999999,1]
["6FX80025DS411CF0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5DS41 4X4 + (2X1.5)C C CONNECTOR FULL THREAD SIZE 1.5 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=15.2 MM LENGTH (M) = 0 + 20 + 5 + 0",906,"TEM",1,"MC",10.377000000000001,1]
["6FX80025DS511BE0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5DS51 4X6 + (2X1.5)C C CONNECTOR FULL THREAD SIZE 1.5 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=17.3 MM LENGTH (M) = 0 + 10 + 4 + 0",742,"TEM",1,"MC",7.7690000000000001,1]
["6FX80025DS541CE0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5DS54 4X6 + (2X1.5)C C CONNECTOR FULL THREAD SIZE 1.5 RING TERMINAL END ON MODULE SID FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=17.3 MM LENGTH (M) = 0 + 20 + 4 + 0",907,"TEM",1,"MC",12.957000000000001,1]
["6FX80025DS641CC0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5DS64 4X10 + (2X1.5)C C CONNECTOR FULL THREAD SIZE 1.5 FOR SINAMICS S120 MOTOR MODULE BOOKSIZE RING TERMINAL END ON MOD. SIDE MOTION-CONNECT 800PLUS TRAIL. TYPE, UL/CSA DESINA, DMAX=20.1 MM LENGTH (M) = 0 + 20 + 2 + 0",1129,"TEM",1,"MC",17.474,1]
["6FX80025DX481AJ0","POWER CABLE, PREASSEMBLED EXT. 4X35+(2X1.5) C, CONN. SIZE 3 (1FT/1FK TO 611/810D/SIMOVERT) TRAILING TYPE UL/CSA DESINA MOTION CONNECT 800 DMAX=32.0 MM, TYPE: 6FX8002-5DX48 LENGTH (M) = 0 + 0 + 8 + 0",2971,"TEM",1,"MC",17.974,1]
["6FX80025DX581AJ0","POWER CABLE EXTENSION 4X50 + (2X1.5)C C, CONNECTOR FULL THREAD SIZE 3 MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=35 MM LENGTH (M) = TYPE: 6FX8002-5DX58 LENGTH (M) = 0 + 0 + 8 + 0",3520,"TEM",1,"MC",23.254000000000001,1]
["6FX80025YW161AF0","POWER CABLE, PREASSEMBLED TYPE: 6FX8002-5YW16 CUSTOM MADE LENGTH (M) = 5",401,"TEM",1,"MC",0.9,1]
["6FX80050BY140SB0","CABLE CUTTING BEAM SET 20/40 6FX8005-0BY14 FIRM BYSTRONIC PARTS LIST NUMBER: 10044325 CONSISTING OF: 6FX8002-5CS01-1AK0 - 10030079 6FX8002-2DC10-1BD0 - 10030115 6FX8002-5CS01-1BD0 - 10030099 6FX8002-2DC10-1BD0 - 10030113",1448,"TEM",1,"MC",5.75,0]
["6FX80081BA312AA0","POWER CABLE,SOLD BY THE METER, TYPE: 6FX8008-1BA31 4X4 + (2X1.5)C C MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 15.2 MM DELIVERY FORM:TIL 79 M IN COILS FROM 80 M DRUM LENGTH (M) = 100 + 0 + 0 + 0",2384,"TEM",1,"MC",33,1]
["6FX80081BA351GD0","POWER CABLE, SOLD BY THE METER, TYPE: 6FX8008-1BA35 4X35 + (2X1.5)C C TRAILING CABLE, UL/CSA DESINA MOTION-CONNECT 800PLUS, DELIV. FORM:UP TO 14 M IN COILS FROM 15 M IN DRUMS DMAX=31.9MM LENGTH (M)= 0 + 60 + 3 + 0",7917,"TEM",1,"MC",126.30200000000001,1]
["6FX80081BA501DA0","POWER CABLE, SOLD BY THE METER, TYPE: 6FX8008-1BA50 4X50 + (2X1.5)C C MOTION-CONNECT 800PLUS, TRAILING CABLE, UL/CSA DESINA DMAX = 35 MM, DELIVERY FORM:TIL 9 M IN COILS FROM 10 M DRUMS LENGTH (M) = 0 + 30 + 0 + 0",5326,"TEM",1,"MC",80.102999999999994,1]
["6FX80081BB311AD0","POWER CABLE,SOLD BY THE METER, TYPE: 6FX8008-1BB31 4X4 C MOTION-CONNECT 800PLUS TRAILING CABLE, UL/CSA DESINA DMAX = 12.3 MM DELIVERY FORM:TIL 99 M IN COILS FROM 100 M  ON DISPOS. DRUM LENGTH (M) = 0 + 0 + 3 + 0",69.5,"TEM",1,"MC",0.93100000000000005,1]
["6FX80081BB411AJ0","POWER CABLE,SOLD BY THE METER, TYPE: 6FX8008-1BB41 4X6.0 C TRAILING CABLE, UL/CSA DESINA MOTION-CONNECT 800PLUS DELIVERY FORM:TIL 69 M IN COILS FROM 70 M DRUM DMAX =14.9 MM, LENGTH (M) = 0 + 0 + 8 + 0",203,"TEM",1,"MC",3.4409999999999998,1]
["6FX80081BB511BH0","POWER CABLE, SOLD BY THE METER TYPE: 6FX8008-1BB51 4X10.0 C TRAILING CABLE, UL/CSA DESINA MOTION-CONNECT 800PLUS DELIVERY FORM:TIL 59 M IN COILS FROM 60 M DRUM DMAX =18,2 MM, LENGTH (M) = 0 + 10 + 7 + 0",590,"TEM",1,"MC",10.711,1]
["6FX80081BB611BG0","POWER CABLE, SOLD BY THE METER, TYPE: 6FX8008-1BB61 4X16 C MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 22.3 MM DELIVERY FORM:TIL 59 M IN COILS AS OF 60 M DRUM LENGTH (M) = 0 + 10 + 6 + 0",722,"TEM",1,"MC",15.201000000000001,1]
["6FX80081BD813AA0","SIGNAL CABLE; SOLD BY THE METER TYPE: 6FX8008-1BD81 12 X 0.22 C MOTION CONNECT 800PLUS TRAILING TYPE, UL/CSA DESINA DELIVERY FORM: IN COILS DMAX = 7.3 MM LENGTH (M) = 200",1269,"TEM",1,"MC",14.34,1]
["6FX80082DC003AA0","SIGNAL CABLE, SOLD BY THE METER TYPE: 6FX8008-2DC00 (DRIVE CLIQ) 2X2X0,2+2X0,38 C, TRAILING TYPE UL/CSA DESINA MOTION CONNECT 800PLUS, DELIVERY FORM: IN COILS DMAX = 7.0 MM, LENGTH (M) = 200",1940,"TEM",1,"MC",14.2,1]
["6FX80122CA311EF0","SIGNAL CABLE, PREASSEMBLED, FOR INCR.ENCODER WITH C/D TRACKS IN MOTOR 3X(2X0.14)C + 4X0,14 + 2X0.5 + 4X0.22 C WITH FULL THREAD CONNECTOR M23 MOTION CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 9.8 MM, LENGTH (M) = TYPE: 6FX8012-2CA31 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = + 0 + 40 + 5 + 0",595,"TEM",1,"MC",4.141,1]
["6FX80122CH001CG0","SIGNAL CABLE, PREASSEMBLED, FOR ABSOLUTE ENCODER ENDAT 6FX2001-5 3X(2X0.14)C + 4X0.14 + 2X0.5 C CONNECTOR FULL THREAD M23 MOTION CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX = 9.2 MM LENGTH (M) = TYPE: 6FX8012-2CH00 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = 0 + 20 + 6 + 0",402,"TEM",1,"MC",2.762,1]
["6FX80125CN011AH5","POWER CABLE PREASSEMBLED 4X1,5 C, SPEED-CONNECT GR. 1 FOR SINAMICS S120 MOTOR MODULE MOTION-CONNECT 800PLUS TRAILING TYPE, UL/CSA, DESINA DMAX=9.5 MM, TYPE: 6FX8012-5CN01 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = + 0 + 0 + 7 + 0,5",348,"TEM",1,"MC",1.42,1]
["6FX80125CS611BA5","POWER CABLE, PREASSEMBLED TYPE: 6FX8012-5CS61 (1FT/1FK/1PH TO SINAMICS) 4X10 C, CONNECTOR SIZE 1.5/10 MM2 TRAILING TYPE, UL/CSA DESINA MOTION-CONNECT 800, MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED DMAX = 19.4 MM, LENGTH (M)= 0 + 10 + 0 + 0,5",700,"TEM",1,"MC",6.9880000000000004,1]
["6FX80125DS011BB0","POWER CABLE, PREASSEMBLED TYPE: 6FX8012-5DS01 (1FT/1FK TO SINAMICS) 4X1.5+(2X1.5)C, CONNECTOR SIZE 1/1.5 MM2 TRAILING TYPE, UL/CSA DESINA MOTION-CONNECT 800, MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED DMAX = 12.9 MM, LENGTH (M)= 0 + 10 + 1 + 0",443,"TEM",1,"MC",2.92,1]
["6FX80125DX381AK0","POWER CABLE EXTENSION 4X25 + (2X1.5)C C CONNECTOR FULL THREAD SIZE 3 MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX=27,6 MM LENGTH (M) = TYPE: 6FX8012-5DX38 MODULE SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = 0 + 0 + 9 + 0",2809,"TEM",1,"MC",15.564,1]
["6FX80425DA051CK0","POWER CABLE, PREASSEMBLED EXT. 4X1.5+(2X1.5)C, CONNECTOR FULL THREAD SIZE 1 MOTION-CONNECT 800PLUS TRAILING TYPE UL/CSA DESINA DMAX= 12 MM, LENGTH (M) = TYPE: 6FX8042-5DA05 MOTOR SIDE: CRIMPED CONTACTS, CONNECTOR HOUSING INCLUDED LENGTH (M) = 0 + 20 + 9 + 0",691,"TEM",1,"MC",7.2220000000000004,1]
["6SE64003CC010BD3","MICROMASTER 4 AC COMMUTATION CHOKE 200V-480V 3AC 9A FOOTPRINT FSB - 2.2MH NOT FOOTPRINT FOR V20",215,"TEM",1,"MC",1.2,1]
["6SE64003TC010BD3","MICROMASTER 4 OUTPUT CHOKE 200V-480V 3AC 10A FOOTPRINT FSB - FSB - 1.243MH NOT FOOTPRINT FOR V20 230V: UP TO 200M CABLE LENGTH 400V: UP TO 150M CABLE LENGTH 480V: UP TO 100M CABLE LENGTH",249,"TEM",1,"MC",3.4,1]
["6SE64202AB155AA1","MICROMASTER 420 WITH BUILT IN CLASS A FILTER 1AC 200-240V +10/-10% 47-63HZ CONSTANT TORQUE POWER   0.55 KW OVERLOAD  150% FOR 60S VARIABLE TORQUE POWER   0.55 KW 173 X 73 X 149 (H X W X D) PROTECTION IP20 AMBIENT TEMP -10 TO +50 DEG C W/O AOP/BOP",420,"TEM",1,"MC",1.3,1]
["6SE64202UD230BA1","MICROMASTER 420 UNFILTERED 3AC 380-480V +10/-10% 47-63HZ CONSTANT TORQUE POWER   3 KW OVERLOAD  150% FOR 60S VARIABLE TORQUE POWER   3 KW 202 X 149 X 172 (H X W X D) PROTECTION IP20 AMBIENT TEMP -10 TO +50 DEG C W/O AOP/BOP",1010,"TEM",1,"MC",3.3,1]
["6SE64402AB112AA1","MICROMASTER 440 WITH BUILT-IN CLASS A FILTER 1AC 200-240 V +10/-10% 47-63 HZ CONSTANT TORQUE POWER  0.12 KW OVERLOAD 150% 60 S, 200% 3 S SQUARED TORQUE POWER  0.12 KW 173 X 73 X 149 (H X W X D) PROTECTION IP20 AMBIENT TEMP. -10 TO +50 DEG. C WITHOUT AOP/BOP",411,"TEM",1,"MC",1.3,1]
["6SE64402UC315DA1","MICROMASTER 440 WITHOUT FILTER 3AC 200-240 V +10/-10% 47-63 HZ CONSTANT TORQUE POWER 15 KW OVERLOAD 150% 60 S, 200% 3 S SQUARED TORQUE POWER 18.5 KW 520 X 275 X 245 (H X W X D) PROTECTION IP20 AMBIENT TEMP. -10 TO +50 DEG. C WITHOUT AOP/BOP",2952,"TEM",1,"MC",16,1]
["6SE64402UE222CA1","MICROMASTER 440 WITHOUT FILTER 3AC 500-600 V +10/-10% 47-63 HZ CONSTANT TORQUE POWER 2.2 KW OVERLOAD 150% 60 S, 200% 3 S SQUARED TORQUE POWER 4 KW 245 X 185 X 195 (H X W X D) PROTECTION IP20 AMBIENT TEMP. -10 TO +50 DEG. C WITHOUT AOP/BOP",1534,"TEM",1,"MC",5.5,1]
["6SE70313FS872DC0","SINAMICS/ SIMOVERT MASTERDRIVES BRAKING RESISTOR 675-780V DC 100 KW, 6.2 OHM",2523,"TEM",1,"MC",43,1]
["6SL30000DE236AA0","SINAMICS HFD LINE REACTOR FOR 36 KW ACTIVE LINE MODULE INPUT: 3AC 380-480 V, 50/60 HZ",1550,"TEM",1,"MC",35.5,1]
["6SL30401LA000AA0","SINAMICS S120 CONTROL UNIT CU310-2 DP WITH PROFIBUS INTERFACE WITHOUT COMPACTFLASH CARD",1271,"TEM",1,"MC",0.95,1]
["6SL30550AA005BA3","SINAMICS S120 SENSOR MODULE SMC20 BOARD FOR EVALUATION OF INCREMENTAL ENCODER: SIN/COS 1VPP ABSOLUTE ENCODER: ENDAT WITHOUT DRIVE-CLIQ CABLE 30 MM WIDTH",413,"TEM",1,"MC",0.63700000000000001,1]
["6SL30750AA000AG0","CAD CREATOR V2.1 MULTILANG.(GE, EN, FR, IT, SP) DVD: WINDOWS 7, VISTA, XP",55.9,"TEM",1,"MC",0.05,1]
["6SL30974AB000DP3","SINAMICS S120 DOCUMENTATION FUNCTIONS MANUAL DRIVE FUNCTIONS EDITION 01/13, French",205,"TEM",1,"MC",3,0]
["6SL30974AC000EP7","SINAMICS S120 DOCUMENTATION EQUIPMENT MANUAL PERFORMANCE PARTS BOOKSIZE EDITION 04/15, Spanish",229,"TEM",1,"MC",2.6,0]
["6SL30974AE000BP3","SINAMICS S120 DOCUMENTATION EQUIPMENT MANUAL PERFORMANCE PARTS CHASSIS EDITION 01/13, English",149,"TEM",1,"MC",1.5,0]
["6SL30974AG000AP4","SINAMICS S120 DOCUMENTATION GETTING STARTED EDITION 07/16, GERMAN",22.8,"TEM",1,"MC",0.2,0]
["6SL30974AH000RP3","SINAMICS S120 DOCUMENTATION EQUIPMENT MANUAL CONTROL UNIT AND SUPPLEMENTARY SYSTEM COMPONENTS EDITION 01/13, Chin. einf.",138,"TEM",1,"MC",1.1000000000000001,0]
["6SL30974AM000BP4","Documentation SINAMICS SINAMICS S120 Chassis Liquid Cooled Power Units Manual Edition 04/2014, English",153,"TEM",1,"MC",1.2,0]
["6SL30974AP000DP4","SINAMICS S120/S150 DOCUMENTATION MANUAL LISTS EDITION 01/13, French",205,"TEM",1,"MC",8.4,0]
["6SL30974AP100EP3","SINAMICS S110 DOCUMENTATION MANUAL LISTS EDITION 06/12, Spanish",198,"TEM",1,"MC",4,0]
["6SL30974AR000PP5","SINAMICS S120 DOCUMENTATION FUNCTIONS MANUAL SAFETY INTEGRATED EDITION 04/14, Russian",188,"TEM",1,"MC",1.5,0]
["6SL30974CA000YG2","SINAMICS Manual Collection DOCUMENTATION ON DVD EDITION 05/13 GERMAN/English/ITALIAN/ FRENCH/Spanish/CHINESE contains also Micromaster docu",66.399999999999991,"TEM",1,"MC",0.1,0]
["6SL31114VE220HA0","SINAMICS S120 COMBI POWER MODULE INPUT: 3AC 400V, 20KW OUTPUT: 3AC 400V,30A,12A,9A,9A FRAME SIZE: COMBI EXTERNAL AIR COOLING SUPPORT OF THE EXTENDED SAFETY INTEGRATED FUNCTIONS",8626,"TEM",1,"MC",21.35,1]
["6SL31212TE210AA4","SINAMICS S120 DOUBLE MOTOR MODULE INPUT: DC 600V OUTPUT: 3AC 400V, 9A/9A FRAME SIZE: BOOKSIZE EXTERNAL AIR COOLING OPTIMIZED PULSE SAMPLE AND SUPPORT OF THE EXTENDED SAFETY INTEGRATED FUNCTIONS INCL. DRIVE-CLIQ CABLE",2341,"TEM",1,"MC",5.8,1]
["6SL31316AE210AA1","SINAMICS S120 SMART LINE MODULE INPUT: 3 AC 380-480 V, 50/60HZ OUTPUT: 600 V DC, 17 A, 10 KW FRAME SIZE: BOOKSIZE EXTERNAL AIR COOLING INCL. CONTROL VOLTAGE ADAPTER AND DRIVE-CLIQ CABLE",1557,"TEM",1,"MC",5.6,1]
["6SL31621AH010AA0","SINAMICS SHIELD CONNECTION SHEET FOR 200 MM LINE/MOTOR MODULES INTERNAL AIR COOLING",35.700000000000003,"TEM",1,"MC",0.55000000000000004,1]
["6SL31638JM000AA0","SINAMICS S120 Terminal Kit ALM 300mm",108,"TEM",1,"MC",0.06,1]
["6SL32020AE220SA0","SINAMICS SINE-WAVE FILTER FOR POWER MODULE FSC FOOT PRINT 3AC 380-480V 20,0A",796,"TEM",1,"MC",12,1]
["6SL32101KE143AB1","SINAMICS G120C RATED POWER 1,5KW WITH 150% OVERLOAD FOR 3 SEC 3AC380-480V +10/-20% 47-63HZ INTEGRATED FILTER CLASS A I/O-INTERFACE: 6DI, 2DO,1AI,1AO SAFE TORQUE OFF INTEGRATED FIELDBUS: USS/ MODBUS RTU; PROTECTION: IP20/ UL OPEN TYPE SIZE: FSA 196X73X203(HXWXD) EXTERNAL 24V",725,"TEM",1,"MC",2.2999999999999998,1]
["6SL32101KE213UB1","SINAMICS G120C RATED POWER  5,5KW WITH 150% OVERLOAD FOR 3 SEC 3AC380-480V +10/-20% 47-63HZ UNFILTERED I/O-INTERFACE: 6DI, 2DO,1AI,1AO SAFE TORQUE OFF INTEGRATED FIELDBUS: USS/ MODBUS RTU PROTECTION: IP20/ UL OPEN TYPE SIZE: FSB 196X100X203(HXWXD) EXTERNAL 24V",1022,"TEM",1,"MC",2.7,1]
["6SL32101KE232AB1","SINAMICS G120C RATED POWER  15,0KW WITH 150% OVERLOAD FOR 3 SEC 3AC380-480V +10/-20% 47-63HZ INTEGRATED FILTER CLASS A I/O-INTERFACE: 6DI, 2DO,1AI,1AO SAFE TORQUE OFF INTEGRATED FIELDBUS: USS/ MODBUS RTU PROTECTION: IP20/ UL OPEN TYPE SIZE: FSC 295X140X203(HXWXD) EXTERNAL 24V",2443,"TEM",1,"MC",5.5,1]
["6SL32101NE210AL0","SINAMICS G120 POWER MODULE PM230 WITH BUILT IN CL. A FILTER PROTECTION IP20 3AC380-480V +10/-10% 47-63HZ OUTPUT LOW OVERLOAD: 4KW FOR 150% 3S,110% 57S,100% 240S AMBIENT TEMP 0 TO +40 DEG C(LO) 292 X 100 X 165 (HXWXD), FSB WITHOUT CONTROL UNIT AND PANEL APPROVED FOR CU240B/E-2 AND CU230P-2 FIRMWARE-VERSION V4.4 NOTE: PM230 DOES NOT SUPPORT SAFETY",734,"TEM",1,"MC",3.4,1]
["6SL32101NE238UG1","SINAMICS G120 POWER MODULE PM230 UNFILTERED PROTECTION IP20 3AC380-480V +10/-10% 47-63HZ OUTPUT LOW OVERLOAD: 18,5KW FOR 150% 3S,110% 57S,100% 240S AMBIENT TEMP 0 TO +40 DEG C(LO) 355 X 140 X 165 (HXWXD), FSC WITHOUT CONTROL UNIT AND PANEL APPROVED FOR CU240B/E-2 AND CU230P-2 FIRMWARE-VERSION V4.4",2114,"TEM",1,"MC",4.95,1]
["6SL32101PC228UL0","SINAMICS POWER MODULE PM240-2 WITHOUT FILTER WITH BUILT IN BRAKING CHOPPER 3AC200-240V +10/-10% 47-63HZ OUTPUT HIGH OVERLOAD: 5,5KW FOR 200% 3S,150% 57S,100% 240S AMBIENT TEMP -10 TO +50 DEG C OUTPUT LOW OVERLOAD: 7,5KW FOR 150% 3S,110% 57S,100% 240S AMBIENT TEMP -10 TO +40 DEG C 355 X 140 X 165 (HXWXD), FSC PROTECTION IP20 WITHOUT CONTROL UNIT AND PANEL APPROVED FOR CU FIRMWARE- VERSION V4.6",1107,"TEM",1,"MC",4.8,1]
["6SL32101PE288AL0","SINAMICS G120 POWER MODULE PM240-2 WITH BUILT IN CL. A FILTER WITH BUILT IN BRAKING CHOPPER 3AC380-480V +10/-20% 47-63HZ OUTPUT HIGH OVERLOAD: 37KW FOR 200% 3S,150% 57S,100% 240S AMBIENT TEMP -20 TO +50 DEG C (HO) OUTPUT LOW OVERLOAD: 45kW FOR 150% 3S,110% 57S,100% 240S AMBIENT TEMP -20 TO +40 DEG C (LO) 551 X 275 X 237 (HXWXD), FSE PROTECTION IP20 WITHOUT CONTROL UNIT AND PANEL APPROVED FOR CU FIRMWARE- VERSION V4.7 HF8",6492,"TEM",1,"MC",32.880000000000003,1]
["6SL32101PH312AL0","SINAMICS G120 POWER MODULE PM240-2 WITH BUILT IN CL. A FILTER WITH BUILT IN BRAKING CHOPPER 3AC500-690V +10/-20% 47-63HZ OUTPUT HIGH OVERLOAD: 90KW FOR 200% 3S,150% 57S,100% 240S AMBIENT TEMP -20 TO +50 DEG C (HO) OUTPUT LOW OVERLOAD: 110kW FOR 150% 3S,110% 57S,100% 240S AMBIENT TEMP -20 TO +40 DEG C (LO) 708 X 305 X 357 (HXWXD), FSF PROTECTION IP20 WITHOUT CONTROL UNIT AND PANEL APPROVED FOR CU FIRMWARE- VERSION V4.7 HF8",13579,"TEM",1,"MC",74,1]
["6SL32101SE260UA0","SINAMICS S120 CONVERTER POWER MODULE PM340 INPUT: 3AC 380-480V, 50/60HZ OUTPUT: 3AC  60A (30KW) FRAME SIZE: BLOCKSIZE SIZE FSD INTERNAL AIR COOLING",5075,"TEM",1,"MC",15.9,1]
["6SL32105BB230AV0","SINAMICS V20 1AC200-240V -10/+10% 47-63HZ RATED POWER 3,0KW WITH 150% OVERLOAD FOR 60SEC INTEGRATED FILTER C2 I/O-INTERFACE: 4DI, 2DO,2AI,1AO FIELDBUS: USS/ MODBUS RTU WITH INBUILT BOP PROTECTION: IP20/ UL OPEN TYPE SIZE:FSC 184X182X169(WXHXD)",460,"TEM",1,"MC",3.2,1]
["6SL32105CC170UA0","SINAMICS V60 CONTROLLED POWER MODULE CPM60.1 INPUT: 3AC 220-240V 50/60HZ OUTPUT: 3AC 7A (1,2 KW)",1007,"TEM",1,"MC",2.63,1]
["6SL32105FE135UF0","SINAMICS V90, WITH PROFINET INPUT: 3AC 380-480V -15%/+10% 13.8A 45-66HZ OUTPUT: 0-INPUT V 11.0A 0-330HZ MOTOR:3.5KW PROTECTION: IP20 FRAME SIZE  C 140X260X240WXHXD",1986,"TEM",1,"MC",6.5149999999999997,1]
["6SL32110KB112UB1","SINAMICS G110 - CPM110 AC-DRIVE, WITHOUT FILTER 1AC200-240V +10/-10% 47-63HZ RS485-INTERFACE (USS-PROTOCOL) CT: 0.12KW; VT: 0.12KW CT-OVERLOAD: 150% 60S 150 X 90 X 101 (HXWXD) IP20; WITH FLAT HEATSINK; COLDPLATE ASSEMBLY ONLY AMBIENT TEMP -10 TO +50 DEG C WITHOUT BOP WITHOUT ANALOG INPUT",209,"TEM",1,"MC",0.6,1]
["6SL32110KB175UB1","SINAMICS G110 - CPM110 AC-DRIVE, WITHOUT FILTER 1AC200-240V +10/-10% 47-63HZ RS485-INTERFACE (USS-PROTOCOL) CT: 0.75KW; VT: 0.75KW CT-OVERLOAD: 150% 60S 150 X 90 X 101 (HXWXD) IP20; WITH FLAT HEATSINK; COLDPLATE ASSEMBLY ONLY AMBIENT TEMP -10 TO +40 DEG C WITHOUT BOP WITHOUT ANALOG INPUT",289,"TEM",1,"MC",0.7,1]
["6SL32230DE137AG1","SINAMICS G120P POWER MODULE PM230 WITH BUILT IN CL. A FILTER PROTECTION IP55 / UL TYPE12 3AC380-480V +10/-10% 47-63HZ OUTPUT LOW OVERLOAD: 0,37KW FOR 150% 3S,110% 57S,100% 240S AMBIE. TEMP -10 TO+40 DEG C(LO) 460 X 154 X 249 (HXBXT), FSA WITHOUT CONTROL UNIT AND PANEL APPROVED FOR CU230P-2 FIRMWARE-VERSION V4.3.2",458,"TEM",1,"MC",4.3,1]
["6SL32230DE315BG1","SINAMICS G120P POWER MODULE PM230 WITH BUILT IN CL. B FILTER PROTECTION IP55 / UL TYPE12 3AC380-480V +10/-10% 47-63HZ OUTPUT LOW OVERLOAD: 15KW FOR 150% 3S,110% 57S,100% 240S AMBIE. TEMP -10 TO+40 DEG C(LO) 620 X 230 X 249 (HXBXT), FSC WITHOUT CONTROL UNIT AND PANEL APPROVED FOR CU230P-2 FIRMWARE-VERSION V4.3.2",2972,"TEM",1,"MC",9.5,1]
["6SL32230DE318AA1","SINAMICS G120P POWER MODULE PM230 WITH BUILT IN CL. A FILTER PROTECTION IP55 / UL TYPE12 3AC380-480V +10/-10% 47-63HZ OUTPUT LOW OVERLOAD: 18,5KW FOR 150% 3S,110% 57S,100% 240S AMBIE. TEMP -10 TO+40 DEG C(LO) 620 X 230 X 249 (HXBXT), FSC WITHOUT CONTROL UNIT AND PANEL APPROVED FOR CU230P-2 FIRMWARE-VERSION V4.3.2",3143,"TEM",1,"MC",9.5,1]
["6SL32250BE345UA0","SINAMICS G120 POWER MODULE PM250 WITHOUT FILTER POSSIBILITY OF REGENERATION 3AC380-480V +10/-10% 47-63HZ OUTPUT HIGH OVERLOAD: 45KW FOR 200% 3S,150% 57S,100% 240S AMBIENT TEMP 0 TO +50 DEG C OUTPUT LIGHT OVERLOAD: 55KW FOR 150% 3S,110% 57S,100% 240S AMBIENT TEMP 0 TO +40 DEG C 634 X 350 X 316 (HXWXD), FSF PROTECTION IP20 WITHOUT CONTROL UNIT AND BOP",8336,"TEM",1,"MC",35,1]
["6SL32550BT010PA0","SINAMICS G120 CHEMICAL INDUST. MODULE CM240NE FOR OPERATION WITH CU240S DP-F CU250S-2 DP ATEX CERTIFIED COLD LEADER EVALUATION,NAMUR TERMINAL STRIP FOR OPERATION WITH CU250S-2 DP THE SUPPLEMENTARY KIT  CM240NE (6SL3260-4TA00-1AA6) IS NEEDED (RAIL MOUNTING)",1796,"TEM",1,"MC",0.8,1]
["6SL32661AB000VA0","SINAMICS V20 FSB SHIELD CONNECTION KIT SIZE: 142X130X27(WXHXD)",26.1,"TEM",1,"MC",0.247,1]
["6SL33151TE321AA3","SINAMICS S120 CONVERTER POWER MODULE 3PH 380-480V, 50/60HZ, 210A (110 KW) FRAME SIZE: CHASSIS LIQUID COOLING INCL. DRIVE-CLIQ CABLE AND MOUNTING PLATE FOR CU310 SUPPORT OF EXTENTED SAFETY INTEGRATED FUNCTIONS",19519,"TEM",1,"MC",76,1]
["6SL34201TE210AA1","SINAMICS S120 SINGLE MOTOR MODULE INPUT: DC 600V OUTPUT: 3AC 400V, 9A FRAME SIZE BOOKSIZE COMPACT INTERNAL AIR COOLING OPTIMIZED PULSE PATTERNS AND HELP HIGHER ORDER SAFETY FUNCTIONS INCL. DRIVE-CLIQ CABLE",1595,"TEM",1,"MC",3,1]
["6SL35326DF710RA2","DISTRIBUTED SERVO-DRIVE SINAMICS S120M AH36, M(0)=1,00Nm, n(n)=3000 RPM, INPUT: DC 600V ABSOLUTE ENCODER 20 BIT NATURAL AIR COOLING, IM B5, IM V1, IM V3 DEGREE OF PROTECTION: IP65 ON SHAFT END IP67 SHAFT WITH FITTED KEY TOLERANCE N; W/O HOLDING BRAKE",3547,"TEM",1,"MC",4.4000000000000004,1]
["6SL35426DF710RH1","DISTRIBUTED SERVO-DRIVE SINAMICS S120M AH48, M(0)=2,5Nm, N(N)=3000 RPM, INPUT: DC 600V ABSOLUTE ENCODER 20 BIT NATURAL AIR COOLING, IM B5, IM V1, IM V3 DEGREE OF PROTECTION: IP65 PLAIN SHAFT WITH HOLDING BRAKE",4174,"TEM",1,"MC",8.1999999999999993,1]
["6SL35552BC100AA0","SINAMICS S120M ADAPTER MODULE 600 FRAME SIZE: BOOKSIZE COMPACT INPUT: DC 600V INTERNAL AIR COOLING",1290,"TEM",1,"MC",4.0650000000000004,1]
["3RA11201CD240BB4","LOAD FEEDER FUSELESS DIRECT STARTING,AC 400V,SIZE S0 1.8...2.5 A, DC 24 V, SCREW CONNECTION ON 60 MM BUSBAR ADAPTER TYPE OF COORDIN. 2, IQ = 50 KA (ALSO COMPATIBLE WITH TYPE OF COORDINATION 1)",186.55,"TEM",1,"CP",1.1100000000000001,1]
["3RA11304GB360AP0","LOAD FEEDER FUSELESS DIRECT STARTING,AC 400V,SIZE S2 36...45 A, AC 230 V, 50 HZ, SCREW CONNECTION, ON ADAPTER FOR SCREW AND SNAP-ON MOUNTING TYPE OF COORDIN. 2, IQ = 50 KA",368.69,"TEM",1,"CP",2.1080000000000001,1]
["3RA14358XC211AL2","CONTACTOR ASSEMBLY, STAR-DELTA (ASSEMBLED) WITH TIME RELAIS AT THE SIDE, AC-3 37KW/400 V, 3-POLE, SIZES S2,S2,S2, EL. LOCKED, SCREW CONNECTION, AC 230V, 50/60 HZ",572.98,"TEM",1,"CP",3.65,1]
["3RA19211D","LINK MODULE ELECTRICAL AND MECHANICAL FOR 3RV1.2 AND 3RT101 FOR 3RV2.1/3RV2.2 AND 3RT2.1 AC AND DC OPERATION (MULTI-UNIT PACKAGING)",5.4,"TEM",1,"CP",0.02,10]
["3RA19411A","LINK MODULE (EL. A. MECH.) FOR 3RV1.41 A. 3RT1.4., 3RW3, PACKING = 5 ITEMS AC OPERATION",13.5,"TEM",1,"CP",0.379,5]
["3RA19632A","CABLE SET FOR REVERSING STARTER MOD. S10",291,"TEM",1,"CP",2.41,1]
["3RA23168XB301AF0","REV. COMB., AC3, 4KW/400V AC110V, 50/60 HZ, 3-POLE, SZ S00 SCREW TERMINAL ELECTR. AND MECH. INTERLOCK",68.27,"TEM",1,"CP",0.495,1]
["3RA24238XF321AC2","STAR-DELTA COMB. AC3, 11KW/400V AC24V, 50/60HZ, 3-POLE, SZ S0, SCREW TERMINAL ELECTR. AND MECH. INTERLOCK 3NO+3NC INTEGR.",254.71,"TEM",1,"CP",1.8620000000000001,1]
["3RA29332C","WIRING KIT ELECTRICAL AND MECHANICAL, F. STAR-DELTA (WYE-D.) S2/S2/S0",22.88,"TEM",1,"CP",0.18,1]
["3RA62501CP32","SIRIUS, COMPACT STARTER, REVERSING STARTER 690 V, 110 ... 240 V AC/DC, 50 ... 60 HZ, 1 ... 4 A, IP20, MAIN CIRCUIT CONNECTION: SCREW TERMINAL, AUXILIARY CIRCUIT CONNECTION: SCREW TERMINAL",432.45,"TEM",1,"CP",2.532,1]
["3RB20161PB0","OVERLOAD RELAY 1...4 A FOR MOTOR PROTECTION SIZE S00, CLASS 10 FOR MOUNTING ONTO CONT. MAIN CIRCUIT: SCREW CONNECTION AUX. CIRCUIT: SCREW CONNECTION MANUAL-AUTOMATIC-RESET",62.7,"TEM",1,"CP",0.19,1]
["3RB20461EB0","OVERLOAD RELAY 25...100 A FOR MOTOR PROTECTION SIZE S3, CLASS 10 FOR MOUNTING ONTO CONT. MAIN CIRCUIT: SCREW CONNECTION AUX. CIRCUIT: SCREW CONNECTION MANUAL-AUTOMATIC-RESET",153.30000000000001,"TEM",1,"CP",0.55000000000000004,1]
["3RB21234QD0","OVERLOAD RELAY 6...25 A FOR MOTOR PROTECTION SIZE S0, CLASS 5...30 FOR MOUNTING ONTO CONT. MAIN CIRCUIT: SCREW CONNECTION AUX. CIRCUIT: SPRINGLOAD. TERM. MANUAL-AUTOMATIC-RESET INT. EARTH FAULT DETECTION",154.9,"TEM",1,"CP",0.2,1]
["3RB21634GC2","OVERLOAD RELAY 55...250 A FOR MOTOR PROTECTION SIZE S10/S12, CLASS 5...30 MOUNT. ONTO CONT./ STAND-ALONE MAIN CIRCUIT: BAR CONNECTION AUX. CIRCUIT: SCREW CONNECTION MANUAL-AUTOMATIC-RESET INT. EARTH FAULT DETECTION",309.10000000000002,"TEM",1,"CP",1.6,1]
["3RB29842","COVER SEALABLE FOR 3RB22/23/24 SIZE S00...S12",7.38,"TEM",1,"CP",4.0000000000000001E-3,10]
["3RB30261QB0","OVERLOAD RELAY 6...25 A FOR MOTOR PROTECTION SIZE S0, CLASS 10 CONTACTOR ASS. MAIN CIRCUIT: SCREW CONN. AUX.CIRCUIT: SCREW CONN. MANUAL-AUTOM.-RESET",58.73,"TEM",1,"CP",0.26,1]
["3RB31134PB0","OVERLOAD RELAY 1...4 A FOR MOTOR PROTECTION SIZE S00, CLASS 5...30 CONTACTOR ASS. MAIN CIRCUIT: SCREW CONN. AUX.CIRCUIT: SCREW CONN. MANUAL-AUTOM.-RESET INT. GROUND FAULT DETECTION",110.19,"TEM",1,"CP",0.22500000000000001,1]
["3RE10208XC260AP0","DIRECT STARTER, 11 KW, RELAY CAN BE CONNECTED, CONTACTOR 3RT10, 230 V, 50 HZ, SIZE S0, PE AND N TERMINAL MOULDED PLASTIC HOUSING IP65, EUROPEAN DESIGN, PUSHB. I-0 (0=R), BLACK/WHITE",135.30000000000001,"TEM",1,"CP",0.82699999999999996,1]
["3RF21201AA04","SEMICONDUCTOR RELAY 3RF2, 1-PH. WIDTH 22.5MM, 20 A 48-460 V / 24 V DC SCREW TERMINAL",37.31,"TEM",1,"CP",7.1999999999999995E-2,1]
["3RF22553AC45","SOLID STATE RELAY 3-PHASE 3RF2 55 A 40 DEG. C 48-600 V / 4-30 V DC 3PH.-CONTROLLED RING TERMINAL LUG BLOCKING VOLTAGE 1200 V",161.13,"TEM",1,"CP",0.14799999999999999,1]
["3RF23202AA04","SEMI-COND. CONTACTOR 3RF2,1-PH. AC 51 20 A   40 DEGREES C 48-460 V / 24 V DC SPRING-LOADED TERMINAL",61.71,"TEM",1,"CP",0.24399999999999999,1]
["3RF23501AA04","SEMI-COND. CONTACTOR 3RF2,1-PH. AC 51 50 A   40 DEGREES C 48-460 V / 24 V DC SCREW TERMINAL",79.44,"TEM",1,"CP",0.54,1]
["3RF34051BB24","SOLID-STATE CONTACTOR 3-PH 3RF3 AC53 5.2A   40 DEGREES C 48-480V / 110-230V AC 2-PH. CONTROLLED INSTANTANEOUS SCREW TERMINALS",132.22999999999999,"TEM",1,"CP",0.31,1]
["3RH11221BD40","CONTACTOR RELAY, 2NO+2NC, DC 42 V, SCREW CONNECTION, SIZE S00",40.6,"TEM",1,"CP",0.26400000000000001,1]
["3RH11222BF40","CONTACTOR RELAY, 2NO+2NC, DC 110 V, CAGE-CLAMP CONNECTION, SIZE S00",37.43,"TEM",1,"CP",0.25800000000000001,1]
["3RH11311BE40","CONTACTOR RELAY, 3NO+1NC, DC 60 V, SCREW CONNECTION, SIZE S00",40.6,"TEM",1,"CP",0.26200000000000001,1]
["3RH11311BG40","CONTACTOR RELAY, 3NO+1NC, DC 125 V, SCREW CONNECTION, SIZE S00",40.6,"TEM",1,"CP",0.25900000000000001,1]
["3RH11401BM40","CONTACTOR RELAY, 4NO, DC 220 V, SCREW CONNECTION, SIZE S00",36.92,"TEM",1,"CP",0.26,1]
["3RH13531DF400KA0","CONTACTOR RELAY,5NO+3NC,110V DC SCREW TERMINAL, SIZE S00, MOUNTED VARISTOR 2NO+2NC BASIC DEVICE /DIN EN 50005",65.180000000000007,"TEM",1,"CP",0.317,1]
["3RH19111BA10","AUX. SWITCH BLOCK, 1NO, DIN EN 50005, CONNECTION FROM BELOW, SCREW CONNECTION, F. CONTACTOR RELAYS A. CONTACT.",5.7,"TEM",1,"CP",0.02,1]
["3RH19111HA01","AUXILIARY SWITCH BLOCK, 11E (1NC), DIN EN50012, SCREW CONNECTION, FOR CONTACTORS FOR SWITCHING MOTORS, 4-POLE",5.8,"TEM",1,"CP",3.5000000000000003E-2,1]
["3RH19112GA22","AUXILIARY SWITCH BLOCK, 62E, 2NO+2NC, DIN EN50011, CAGE CLAMP CONNECTION FOR CONTACTOR RELAYS, 4-POLE",12.8,"TEM",1,"CP",5.8999999999999997E-2,1]
["3RH19211FA04","MOUNTING BLOCK DIN EN 50005, 4-POLE, 4NC",11.7,"TEM",1,"CP",7.3999999999999996E-2,1]
["3RH19211PA22","AUX. CONT. BLOCK, 22 (2NO+2NC) DIN EN50005, 4-POLE, SCREW CONNECTION,FRONTSEITIG FOR MOTOR CONTAC. SIZE S0...S3",11.7,"TEM",1,"CP",7.4999999999999997E-2,1]
["3RH19212HA31","AUXILIARY SWITCH BLOCK, 31 (3NO+1NC), DIN EN50005, CAGE CLAMP CONNECTION, FOR CONTACTORS FOR SWITCHING MOTORS, 4-POLE",12,"TEM",1,"CP",7.1999999999999995E-2,1]
["3RH21221BM40","CONTACTOR RELAY, 2NO+2NC, DC 220V, SIZE S00, SCREW TERMINAL",31.26,"TEM",1,"CP",0.29299999999999998,1]
["3RH21402AF00","CONTACTOR RELAY, 4NO, AC 110V, 50/60 HZ, SZ S00, SPRING-LOADED TERMINAL",27.06,"TEM",1,"CP",0.254,1]
["3RH24401BB40","CONTACTOR RELAY LATCHED, 4NO, DC 24V, SIZE S00, SCREW TERMINAL",97.68,"TEM",1,"CP",0.55400000000000005,1]
["3RH29111GA40","AUX.SWITCH BLOCK,FRONT,4NO, CURR.PATH: 1NO, 1NO, 1NO, 1NO, FOR CONTACTOR RELAYS, SZ S00, SCREW TERMINAL 53 / 54,63 / 64,73 / 74,83 / 84 F. 3RH2140 / 3RH2440 (EN 50011)",13.31,"TEM",1,"CP",5.1999999999999998E-2,1]
["3RK11051AE040CA0","ASISAFE BASIC SAFETY MONITOR 1 F-RO, 1 ENABLING CIRCUIT, IP20, WITH SCREW-TYPE TERMINALS (REMOVABLE), SAFE OUTPUT RELAY RESPONSE TIME MAX. 40 MS, MONITOR TYPE 1, VERSION 3, APPLICABLE UP TO CATEGORY 4 (EN 954-1), UP TO PL E (EN ISO 13849-1), UP TO SIL 3 (IEC 61508), FOR AS-INTERFACE / AS-I SAFETY AT WORK",615,"TEM",1,"CP",0.34499999999999997,1]
["3RK13010BB000AA2","DS1-X FOR ET 200S ELECTROMECHANICS LINE STARTER EXPANDABLE ADJUSTABLE RANGE 0.14...0.20A AC-3, TO 0.06 KW/400V FOR BRAKE CONTROL MODULE",246.82,"TEM",1,"CP",0.88800000000000001,1]
["3RK13011CB000AA2","DS1-X FOR ET 200S ELECTROMECHANICS LINE STARTER EXPANDABLE ADJUSTABLE RANGE 1.8...2.5A AC-3, 0.9 KW/400V FOR BRAKE CONTROL MODULE",246.82,"TEM",1,"CP",0.88200000000000001,1]
["3RK13156KS410AA0","SIRIUS MOTOR STARTER M200D AS-I COMMUNICATION: AS-INTERFACE DIRECT ON-LINE STARTER, BASIC MECHANICAL SWITCHING 3 400V AC/0,9KW;0,15A...2,00A; ELECTR. OVERLOAD PROTECTION; THERMISTOR:THERMOCLICK / PTC WITHOUT BRAKE CONTACT 2DI AS-I + 2DI / 1DO ON DEVICE HAN Q4/2 - HAN Q8/0",708.04,"TEM",1,"CP",3.7,1]
["3RK18022FB060GA1","ASISAFE CD (V3) FOR AS-I SAFETY MONITOR, INCLUDES CONFIGURATIONS SOFTWARE ASIMON V3,",189.83,"TEM",1,"CP",0.216,1]
["3RK19015AA00","CABLE SET AS-I SAFETY MONITOR, INCLUDES 1 PC CONFIGURATION CABLE FOR COMMUNICATION BETWEEN PC (SERIAL INTERFACE) AND SAFETY MONITOR, LENGTH ABOUT 150 CM, AND 1 TRANSFERRING CABLE BETWEEN TWO SAFETY MONITORS, LENGTH ABOUT 25 CM",77.489999999999995,"TEM",1,"CP",8.5000000000000006E-2,1]
["3RK19030AC00","TERMINAL MODULE FOR ET 200S RS FOR REVERSING STARTER, WITH FEEDER CONNECTION",162.16,"TEM",1,"CP",0.49,1]
["3RK19031BA00","PM-D F1 F. MOTOR STARTER POWER MODULE, FAILSAFE UP TO SAFETY CAT. 4 EN954-1 FOR MONIT. START EM. STOP PLUGABLE ONTO TM-PF30 S47-B0 -B1 30MM",280.44,"TEM",1,"CP",0.251,1]
["3RK19033EC00","65 MM TERMINAL MODULE FOR ET 200S INVERTER POWER MODULE IPM25 FS A WITH FEEDER CONNECTION",171.69,"TEM",1,"CP",0.55000000000000004,1]
["3RK32421AA10","SIRIUS, EXPANSION MODULE 3RK32 FOR 3RK3 MODULAR SAFETY SYSTEM 4 F-DO, DC 24V/ 2 A PARAMETERIZABLE VIA SW MSS ES 22.5MM WIDTH SCREW TERMINAL UP TO SIL3 (IEC 61508) UP TO PERFORMANCE LEVEL E (ISO 13849-1)",492.41,"TEM",1,"CP",0.19,1]
["3RM12021AA14","MOTOR STARTER SIRIUS 3RM1 REVERSING STARTER 500 V; 0,4-2,0 A; 110-230 V AC SCREW CONNECTION SYSTEM",152.62,"TEM",1,"CP",0.33300000000000002,1]
["3RN10101CM00","THERMISTOR MOTOR PROTECTION STANDARD EVALUATION UNIT AUTO, 1NO+1NC, AC230V SCREW CONNECTION",72.06,"TEM",1,"CP",0.16800000000000001,1]
["3RN10131BW10","THERMISTOR MOTOR PROTECTION MULTIFUNCTION EVALUATION UNIT MANUAL/AUTO/REMOTE, SHORT-CIRC.DETECT., 2W, UC 24...240V, SCREW CONNECTION",184.19,"TEM",1,"CP",0.16500000000000001,1]
["3RP25121AW30","TIME RELAY, ELECTRONIC, DELAYED, 1 CO CONT., 1 TIME RANGE 1.5S...30S, 12...240V AC/DC AT AC 50/60HZ, LED, SCREW TERMINAL",50.09,"TEM",1,"CP",0.13600000000000001,1]
["3RR21421AW30","MONITORING RELAY ATTACHABLE TO CONTACTOR 3RT2. SIZE S0 BASIC, ANALOG ADJUSTABLE APPARENT CURRENT MONITORING 4 - 40A, 50-60 HZ, 2-PHASE SUPPLY 24-240 V AC/DC 1 CO CONTACT MONITORING FOR CURRENT OVERSHOOT/UNDERSHOOT PHASE FAILURE, WIRE BREAK WITH OR W/O ERROR LOG ON-DELAY 0-60 S SPURIOUS PEAK SUPPR.0-30 S SWITCHING HYSTERESIS 6% SCREW CONNECTION",108.04,"TEM",1,"CP",0.30299999999999999,1]
["3RS10421GW70","TEMPERATURE MONITORING RELAY PT100/1000 KTY83/84, NTC, 2 THRESHOLDS, DIGITAL, -50 DEGREES C TO 750 DEGREES C (SENSOR-DEPENDENT), 24 V TO 240 V AC/DC, 2 X 1 CO + 1 NO,  WIDTH 45 MM, SCREW TERMINAL",291.31,"TEM",1,"CP",0.30199999999999999,1]
["3RS70051FE00","SIGNAL CONVERTER 24 V AC/DC, 3-WAY ISOLATION IN: 0 TO 10 V, 0/4 TO 20 MA OUT: 0 TO 10 V, 0/4 TO 20 MA SCREW TERMINAL",162.26,"TEM",1,"CP",4.8000000000000001E-2,1]
["3RT10151AV01","CONTACTOR, AC-3 3 KW/400 V, 1 NO, AC 400 V, 50/60 HZ, 3-POLE, SIZE S00, SCREW CONNECTION",31.72,"TEM",1,"CP",0.20100000000000001,1]
["3RT10152AF01","CONTACTOR, AC-3 3 KW/400 V, 1 NO, AC 110 V, 50/60 HZ, 3-POLE, SIZE S00, CAGE CLAMP CONNECTION",29.48,"TEM",1,"CP",0.20399999999999999,1]
["3RT10161AN21","CONTACTOR, AC-3 4 KW/400 V, 1 NO AC 220V 50/60HZ, 3-POLE, SIZE S00, SCREW CONNECTION",31.11,"TEM",1,"CP",0.20200000000000001,1]
["3RT10161BM41","CONTACTOR, AC-3 4 KW/400 V, 1 NO, DC 220 V, 3-POLE, SIZE S00, SCREW CONNECTION",36.11,"TEM",1,"CP",0.25900000000000001,1]
["3RT10162BB41","CONTACTOR, AC-3 4 KW/400 V, 1 NO, DC 24 V, 3-POLE, SIZE S00, CAGE CLAMP",36.520000000000003,"TEM",1,"CP",0.26300000000000001,1]
["3RT10171AP01","CONTACTOR, AC-3 5.5 KW/400 V, 1 NO, AC 230 V, 50/60 HZ, 3-POLE, SIZE S00, SCREW CONNECTION",34.58,"TEM",1,"CP",0.20300000000000001,1]
["3RT10171KB42","COUPLING RELAY, AC-3 5,5 KW/400 V, 1 NC, DC 24 V, 0.7...1.25*US, W. VARISTOR, 3-POLE, SIZE S00, SCREW CONNECTION",44.68,"TEM",1,"CP",0.26100000000000001,1]
["3RT10231AF04","CONTACTOR, AC-3 4KW/400V, AC 110V, 50HZ, 3-POLE, SIZE S0, SCREW CONNECTION WITH 2NO+2NC",46.92,"TEM",1,"CP",0.40600000000000003,1]
["3RT10241AB04","CONTACTOR, AC-3 5.5 KW/400 V, AC 24 V, 50 HZ, 3-POLE, 2 NO + 2 NC, SIZE S0, SCREW CONNECTION",48.86,"TEM",1,"CP",0.41199999999999998,1]
["3RT10241AV00","CONTACTOR, AC-3 5,5 KW/400 V, AC 400 V 50 HZ, 3-POLE, SIZE S0, SCREW CONNECTION",35.090000000000003,"TEM",1,"CP",0.33700000000000002,1]
["3RT10251AB04","CONTACTOR, AC-3 7.5 KW/400 V, AC 24 V, 50 HZ, 3-POLE, 2 NO + 2 NC, SIZE S0, SCREW CONNECTION",64.260000000000005,"TEM",1,"CP",0.41299999999999998,1]
["3RT10251BB44","CONTACTOR, AC-3 7.5 KW/400 V, DC 24 V, 3-POLE, 2 NO + 2 NC, SIZE S0, SCREW CONNECTION",103.94,"TEM",1,"CP",0.64300000000000002,1]
["3RT10261AC20","CONTACTOR, AC-3 11 KW/400 V, AC 24V 50/60HZ, 3-POLE, SIZE S0, SCREW CONNECTION",62.73,"TEM",1,"CP",0.33800000000000002,1]
["3RT10263AP00","CONTACTOR, AC-3 11 KW/400 V, AC 230 V, 50 HZ, 3-POLE, SIZE S0, CAGE CLAMP",63.85,"TEM",1,"CP",0.33800000000000002,1]
["3RT10263BB40","CONTACTOR, AC-3 11 KW/400 V, DC 24 V, 3-POLE, SIZE S0, CAGE CLAMP",103.94,"TEM",1,"CP",0.56799999999999995,1]
["3RT10343AP00","CONTACTOR, AC-3 15 KW/400 V, AC 230 V, 50 HZ, 3-POLE, SIZE S2, CAGE CLAMP",92.56,"TEM",1,"CP",0.81100000000000005,1]
["3RT10351AL24","CONTACTOR, AC-3 18,5 KW/400 V, AC 230V 50/60HZ, 2 NO + 2 NC 3-POLE, SIZE S2, SCREW CONNECTION",126.59,"TEM",1,"CP",0.93600000000000005,1]
["3RT10361AC20","CONTACTOR, AC-3 22 KW/400 V, AC 24V 50/60HZ, 3-POLE, SIZE S2, SCREW CONNECTION",116.24,"TEM",1,"CP",0.84699999999999998,1]
["3RT10361AQ20","CONTACTOR 3-PH 22 KW/400 V, 500 V AC, 50/60 HZ, 3-POLE, SIZE S2, SCREW CONNECTION",119.21,"TEM",1,"CP",0.84599999999999997,1]
["3RT10441AB00","CONTACTOR, AC-3 30 KW/400 V, AC 24 V, 50 HZ, 3-POLE, SIZE S3, SCREW CONNECTION",160.82,"TEM",1,"CP",1.7110000000000001,1]
["3RT10441AN24","CONTACTOR, AC-3 30 KW/400 V, AC 220V 50/60HZ 2 NO + 2 NC 3-POLE, SIZE S3, SCREW CONNECTION",175.48,"TEM",1,"CP",1.79,1]
["3RT10443AF00","CONTACTOR, AC-3 30 KW/400 V, AC 110 V, 50 HZ, 3-POLE, SIZE S3, CAGE CLAMP",163.80000000000001,"TEM",1,"CP",1.7170000000000001,1]
["3RT10451AP60","CONTACTOR, AC-3 37 KW/400 V, AC 220V 50HZ/240V 60HZ 3-POLE, SIZE S3, SCREW CONNECTION",230.22,"TEM",1,"CP",1.8420000000000001,1]
["3RT10461AB00","CONTACTOR, AC-3 45 KW/400 V, AC 24 V, 50 HZ, 3-POLE, SIZE S3, SCREW CONNECTION",283.11,"TEM",1,"CP",1.8480000000000001,1]
["3RT10463AF00","CONTACTOR, AC-3 45 KW/400 V, AC 110 V, 50 HZ, 3-POLE, SIZE S3, CAGE CLAMP",288.13,"TEM",1,"CP",1.839,1]
["3RT10546AB36","CONTACTOR, 55KW/400V/AC-3, AC(40...60HZ)/DC OPERATION UC 23...26V AUX. CONTACTS 2NO+2NC, 3-POLE, SIZE S6 BAR CONNECTIONS CONVENTIONAL OPERATING MECHAN. SCREW TERMINAL",331.5,"TEM",1,"CP",3.29,1]
["3RT10556NP36","CONTACTOR, 75KW/400V/AC-3, AC(40...60HZ)/DC OPERATION UC 200...277V AUXIL. CONTACTS 2NO+2NC 3-POLE, SIZE S6 BAR CONNECTIONS ELECTRONIC OPERATING MECHANISM WITH PLC INTERFACE 24V DC SCREW TERMINAL",428.4,"TEM",1,"CP",3.3250000000000002,1]
["3RT10652AP36","CONTACTOR, 132KW/400V/AC-3 AC(40...60HZ)/DC OPERATION UC 220-240V AUXILIARY CONTACTS 2NO+2NC 3-POLE, SIZE S10 BAR CONNECTIONS CONVENT. OPERATING MECHANISM CAGE CLAMP TERMINAL",837.7,"TEM",1,"CP",6.5,1]
["3RT10666NP36","CONTACTOR, 160KW/400V/AC-3 AC(40...60HZ)/DC OPERATION UC 200-277V AUXILIARY CONTACTS 2NO+2NC 3-POLE, SIZE S10 BAR CONNECTIONS ELECTRONIC OPERATING MECHANISM WITH 24V DC PLC INTERFACE SCREW TERMINAL",1041.3,"TEM",1,"CP",6.61,1]
["3RT13171BB40","CONTACTOR, AC-1, 14.5 KW/400V, AC-1 22 A, DC 24 V 4-POLE, 4 NO, SIZE S00, SCREW CONNECTION",42.13,"TEM",1,"CP",0.26500000000000001,1]
["3RT13251AB00","CONTACTOR, AC-1 35 A, AC 24 V 50 HZ 4-POLE, SIZE S0, SCREW CONNECTION",53.45,"TEM",1,"CP",0.39300000000000002,1]
["3RT14766AP36","CONTACTOR, 690A/AC-1 AC(40...60HZ)/DC OPERATION UC 220-240V AUXILIARY CONTACTS 2NO+2NC 3-POLE, SIZE S12 BAR CONNECTIONS CONVENT. OPERATING MECHANISM",1362.3,"TEM",1,"CP",10.366,1]
["3RT15261AF00","CONTACTOR, AC-3 40 A,11KW/400V, AC 110 V, 50 HZ, 4-POLE, 2NO + 2NC, SIZE S0, SCREW CONNECTION",77.209999999999994,"TEM",1,"CP",0.39,1]
["3RT16271AF01","CAPACITOR SW. CONTACTOR, AC-6, 25KVAR/400V, 110V, 50HZ, 3-POLE, SIZE S0",108.22,"TEM",1,"CP",0.43,1]
["3RT19161CC00","RC-ELEMENT, AC 48...127 V, DC 70...150V, SURGE SUPPRESSOR, FOR MOUNTING ONTO CONTACTORS  SIZES00",7.5,"TEM",1,"CP",8.9999999999999993E-3,1]
["3RT19245AB01","COIL FOR CONTACTORS SIRIUS, SIZE S0, SCREW CONNECTION AC 24 V, 50 HZ",16.8,"TEM",1,"CP",9.2999999999999999E-2,1]
["3RT19261CD00","RC ELEMENT, AC 127...240V, DC 150...250V, SURGE SUPPRESSOR, FOR MOUNTING ONTO CONTACTORS SZ. S0,",10.4,"TEM",1,"CP",1.2E-2,1]
["3RT19263AB31","MECHANICAL LATCHING BLOCK FOR MOUNTING ON 3RT1.2. AND 3RT1.3., 24 V AC/DC",63.1,"TEM",1,"CP",0.127,1]
["3RT19346A","EQUIV. CONTACTS F. CONTACTOR SIZE S2, 3-POLE, AC-3, 15 KW, 3 NO, MAIN CONTACTS, CONSISTS OF 3 MOVABLE AND 6 FIXED CONTACTS WITH MOUNTING ACC.",49.5,"TEM",1,"CP",4.2000000000000003E-2,1]
["3RT19361CE00","RC ELEMENT, AC 240...400 V, SURGE SUPPRESSOR, FOR MOUNTING ONTO CONTACTORS FOR S2 AND S3",15.1,"TEM",1,"CP",3.1E-2,1]
["3RT19455AG21","COIL FOR CONTACTORS SIRIUS, SIZE S3, SCREW CONNECTION, AC 110 V, 50/60 HZ",50.8,"TEM",1,"CP",0.17499999999999999,1]
["3RT19555AB31","WITHDR. COIL FOR MOD. S6 FOR CONTACTORS 3RT105/3RT145 AC/DC ACTUATOR  UC23-26V DRIVE: CONVENTIONAL",82.5,"TEM",1,"CP",0.56999999999999995,1]
["3RT19564EA2","TERMINAL COVER FOR BOX TERMINAL BLOCK FOR CONTACTOR SIZE S6, 3RT1.5 FOR OVERLOAD RELAY 3RB105 FOR SOFT STARTER 3RW405., 3RW442., 3RW443.",10.8,"TEM",1,"CP",2.1000000000000001E-2,1]
["3RT19664G","FRAME TERMINAL BLOCK FOR CONTACTORS SIZE S10/S12 FOR OVERLOAD RELAY 3RB106",93.6,"TEM",1,"CP",0.69399999999999995,1]
["3RT20151AP01","CONTACTOR, AC-3, 3KW/400V, 1NO, AC 230V, 50/60 HZ, 3-POLE, SZ S00 SCREW TERMINAL",24.18,"TEM",1,"CP",0.23,1]
["3RT20161AD02","CONTACTOR, AC-3, 4KW/400V, 1NC, AC 42V, 50/60 HZ, 3-POLE, SZ S00 SCREW TERMINAL",27.71,"TEM",1,"CP",0.23,1]
["3RT20171AP61","CONTACTOR, AC-3, 5.5KW/400V, 1NO, AC 220V 50HZ 240V 60 HZ, 3-POLE, SZ S00 SCREW TERMINAL",29.1,"TEM",1,"CP",0.23599999999999999,1]
["3RT20181AP02","CONTACTOR, AC-3, 7.5KW/400V, 1NC, AC 230V, 50/60 HZ, 3-POLE, SZ S00 SCREW TERMINAL",38.729999999999997,"TEM",1,"CP",0.23499999999999999,1]
["3RT20241AB00","CONTACTOR, AC-3, 5.5KW/400V, 1NO+1NC, AC 24V 50HZ, 3-POLE, SZ S0 SCREW TERMINAL",31.21,"TEM",1,"CP",0.40899999999999997,1]
["3RT20241AP00","CONTACTOR, AC-3, 5.5KW/400V, 1NO+1NC, AC 230V 50HZ, 3-POLE, SZ S0 SCREW TERMINAL",31.21,"TEM",1,"CP",0.40699999999999997,1]
["3RT20251AP00","CONTACTOR, AC-3, 7.5KW/400V, 1NO+1NC, AC 230V 50HZ, 3-POLE, SZ S0 SCREW TERMINAL",43.25,"TEM",1,"CP",0.40500000000000003,1]
["3RT20261AH00","CONTACTOR, AC-3, 11KW/400V, 1NO+1NC, AC 48V 50HZ, 3-POLE, SZ S0 SCREW TERMINAL",58.55,"TEM",1,"CP",0.41599999999999998,1]
["3RT20262AP00","CONTACTOR, AC-3, 11KW/400V, 1NO+1NC, AC 230V 50HZ, 3-POLE, SZ S0 SPRING-LOADED TERMINAL",58.55,"TEM",1,"CP",0.44900000000000001,1]
["3RT20272AF00","CONTACTOR, AC-3, 15KW/400V, 1NO+1NC, AC 110V 50HZ, 3-POLE, SZ S0 SPRING-LOADED TERMINAL",81.91,"TEM",1,"CP",0.46100000000000002,1]
["3RT20351AB00","CONTACTOR,AC3:18.5KW/400V, 1NO+1NC, 24V AC 50HZ, 3-POLE, SIZE S2, SCREW TERMINAL",101.33,"TEM",1,"CP",0.98399999999999999,1]
["3RT20371AG20","CONTACTOR,AC3:30KW/400V, 1NO+1NC, 110V AC 50/60HZ, 3-POLE, SIZE S2, SCREW TERMINAL",158.57,"TEM",1,"CP",0.98799999999999999,1]
["3RT23371AP00","4NO CONTACTOR,AC1:110A 230V AC 50HZ, 4-POLE, 4NO, SIZE S2, SCREW TERMINAL 1NO+1NC INTEGRATED",240.32,"TEM",1,"CP",1.147,1]
["3RT26281AP05","CONTACTOR, AC-6B, 33KVAR/400V, 1NO+2NC, 230 V AC 50HZ 3-POLE, SIZE S0 SCREW TERMINAL",130.25,"TEM",1,"CP",0.64700000000000002,1]
["3RT29245AD01","MAGNET COIL F. CONTACTORS 7,5KW AC 42V, 50HZ FOR MOTOR CONTACTORS SZ S0, SCREW TERMINAL,",20.239999999999998,"TEM",1,"CP",7.3999999999999996E-2,1]
["3RU11160CB1","OVERLOAD RELAY, 0.18...0.25 A, 1NO+1NC, SIZE S00, CLASS 10, FOR INDIVID. MOUNTING",49.02,"TEM",1,"CP",0.17399999999999999,1]
["3RU11160FB0","OVERLOAD RELAY, 0.35...0.5 A, 1NO+1NC, SIZE S00, CLASS 10, FOR CONTACTOR MOUNTING",38.24,"TEM",1,"CP",0.155,1]
["3RU11161DB1","OVERLOAD RELAY, 2.2...3.2 A 1NO+1NC, SIZE S00, CLASS 10, FOR INDIVID. MOUNTING",49.02,"TEM",1,"CP",0.18,1]
["3RU11264DB1","OVERLOAD RELAY, 20...25 A, 1NO+1NC, SIZE S0, CLASS 10, SCREW CONNECTION, FOR INDIVID. MOUNTING",50.88,"TEM",1,"CP",0.26,1]
["3RU11364GB1","OVERLOAD RELAY, 36...45 A, 1NO+1NC, SIZE S2, CLASS 10, SCREW CONNECTION, FOR INDIVID. MOUNTING",90.49,"TEM",1,"CP",0.48,1]
["3RU19001C","CABLE RELEASE WITH HOLDER FOR 3RU11/3RB20/3RB21 SIZE S00...S12",36.9,"TEM",1,"CP",7.6999999999999999E-2,1]
["3RU21160JB0","OVERLOAD RELAY 0.70...1.0 A FOR MOTOR PROTECTION SZ S00, CLASS 10, F. MOUNTING ONTO CONTACTOR MAIN CIRCUIT: SCREW TERMINAL AUX. CIRCUIT: SCREW TERMINAL MANUAL-AUTOMATIC-RESET",35,"TEM",1,"CP",0.14499999999999999,1]
["3RU21161KB1","OVERLOAD RELAY 9.0...12.5 A FOR MOTOR PROTECTION BGR S00, CLASS 10 STAND-ALONE INSTALLATION MAIN CIRCUIT: SCREW TERMINAL AUXILARY CIRCUIT:SCREW TERMINAL MANUAL-AUTOMATIC-RESET",44.8,"TEM",1,"CP",0.185,1]
["3RU21264AB0","OVERLOAD RELAY 11...16 A FOR MOTOR PROTECTION SZ S0, CLASS 10, F. MOUNTING ONTO CONTACTOR MAIN CIRCUIT: SCREW TERMINAL AUX. CIRCUIT: SCREW TERMINAL MANUAL-AUTOMATIC-RESET",37.4,"TEM",1,"CP",0.183,1]
["3RU21364EB0","OVERLOAD RELAY 22...32 A FOR MOTOR PROTECTION SIZE S2, CLASS 10 FOR MOUNTING ONTO CONTACTORS MAIN CIRCUIT: SCREW TERMINAL AUX. CIRCUIT: SCREW TERMINAL MANUAL-AUTOMATIC-RESET.",67.400000000000006,"TEM",1,"CP",0.32200000000000001,1]
["3RV10110FA10","CIRCUIT-BREAKER SIZE S00, FOR MOTOR PROTECTION, CLASS 10, A-REL.0.35...0.5A, N-REL.6.5A SCREW TERMINAL, STANDARD SWITCHING CAPACITY",45.31,"TEM",1,"CP",0.23100000000000001,1]
["3RV10111DA10","CIRCUIT-BREAKER SIZE S00, FOR MOTOR PROTECTION, CLASS 10, A-REL.2.2...3.2A, N-REL. 42A, SCREW TERMINAL, STANDARD SWITCHING CAPACITY",50.23,"TEM",1,"CP",0.27900000000000003,1]
["3RV10210CA10","CIRCUIT-BREAKER, 0.18...0.25A N-RELEASE 3,3 A, SIZE S0, MOTOR PROTECTION, CLASS 10, SCREW CONNECTION STANDARD BREAKING CAPACITY",48.79,"TEM",1,"CP",0.28799999999999998,1]
["3RV10211BA10","CIRCUIT-BREAKER SIZE S0, FOR MOTOR PROTECTION, CLASS 10, A-REL. 1.4...2A, N-REL. 26A, SCREW TERMINAL, STANDARD SWITCHING CAPACITY",53.81,"TEM",1,"CP",0.35699999999999998,1]
["3RV10211JA10","CIRCUIT-BREAKER SIZE S0, FOR MOTOR PROTECTION, CLASS 10, A-REL. 7...10A, N-REL. 130A, SCREW TERMINAL, STANDARD SWITCHING CAPACITY",59.86,"TEM",1,"CP",0.36399999999999999,1]
["3RV10314BA10","CIRCUIT-BREAKER 14...20 A, N-RELEASE 260 A, SIZE S2, MOTOR PROTECTION CLASS 10 SCREW CONNECTION STANDARD BREAKING CAPACITY",109.8,"TEM",1,"CP",1.0609999999999999,1]
["3RV10314GA15","CIRCUIT-BREAKER, SIZE S2, FOR MOTOR PROTECTION, CLASS 10, A-RES. 36...45 A, N-RES. 540 A, 1 NO + 1 NC TRANSVERSE, SCREW CONNECTION, STANDARD SWITCHING CAPACITY",183,"TEM",1,"CP",1.073,1]
["3RV10414LA15","CIRCUIT-BREAKER, SIZE S3, FOR MOTOR PROTECTION, CLASS 10, A-RES. 70...90 A, N-RES. 1170 A 1 NO + 1 NC TRANSVERSE, SCREW CONNECTION, STANDARD SWITCHING CAPACITY",236.7,"TEM",1,"CP",2.2839999999999998,1]
["3RV10424MB10","CIRCUIT-BREAKER SIZE S3 A-RELEASE 80...100 A, N-RELEASE 1235 A, MOTOR PROTECTION UP TO 100 KA, CLASS 20, SCREW CONNECTION INCREASED BREAKING CAPACITY",357.4,"TEM",1,"CP",2.3039999999999998,1]
["3RV11314GA10","CIRCUIT-BREAKER, SIZE S2, FOR MOTOR PROTECTION, CLASS 10, WITH OVERLOAD RELAY FUNCTION A REL.36...45A, N REL.585A, SCREW CONNECTION, STANDARD BREAKING CAPACITY",214.5,"TEM",1,"CP",1.125,1]
["3RV13211GC10","CIRCUIT-BREAKER N-RELEASE  82 A, SIZE S0, STARTER PROTECTION, 100 KA, SCREW CONNECTION STANDARD BREAKING CAPACITY",52.07,"TEM",1,"CP",0.35799999999999998,1]
["3RV13314GC10","CIRCUIT-BREAKER N-RELEASE  585 A, SIZE S2 STARTER PROTECTION, 50 KA SCREW CONNECTION STANDARD BREAKING CAPACITY",169,"TEM",1,"CP",1.048,1]
["3RV14210AA10","CIRCUIT-BREAKER, 0.11...0.16A N-RELEASE  3,3A, SIZE S0, TRANSFORMER PROTECTION, CL. 10, SCREW CONNECTION STANDARD BREAKING CAPACITY",53.81,"TEM",1,"CP",0.28599999999999998,1]
["3RV14314BA10","CIRCUIT-BREAKER, 14...20 A N-RELEASE  416 A, SIZE S2 TRANSFORMER PROTECTION, CL. 10, 50KA, SCREW CONNECTION STANDARD BREAKING CAPACITY",125.4,"TEM",1,"CP",1.048,1]
["3RV19011F","TRANSVERSE AUXILIARY SWITCH WITH SCREW CONNECTION, 2NO",7.28,"TEM",1,"CP",1.7999999999999999E-2,1]
["3RV19021DV0","SHUNT TRIP AC 350...415V, 50/60HZ, 100% ED FOR CIRCUIT-BREAKERS, SIZE S00...S3,",23.88,"TEM",1,"CP",0.13200000000000001,1]
["3RV19155DB","CONNECTING PIECE FOR 3-PHASE BUSBARS MODULAR SPACING 45MM",8,"TEM",1,"CP",4.4999999999999998E-2,1]
["3RV19234B","MOULDED PLASTIC FRONT PLATE, IP55, WITH ROTARY OPERATING MECHANISM,  LOCKABLE, FOR CIRCUIT-BREAKER S00,S0,S2,S3",11.28,"TEM",1,"CP",0.10199999999999999,1]
["3RV19462B","DOOR-COUPL. ROT. OPER. MECHAN. FOR CIRCUIT-BREAKERS SIZE S3, GREY HANDLE",81.900000000000006,"TEM",1,"CP",1.722,1]
["3RV20110JA15","CIRCUIT-BREAKER SZ S00, FOR MOTOR PROTECTION, CLASS 10, A-REL. 0.7...1A, N-RELEASE 13A, SCREW CONNECTION, STANDARD SW. CAPACITY, W. TRANSVERSE AUX. SWITCH 1NO+1NC",56.07,"TEM",1,"CP",0.35599999999999998,1]
["3RV20111AA15","CIRCUIT-BREAKER SZ S00, FOR MOTOR PROTECTION, CLASS 10, A-REL.1.1...1.6A, N-RELEASE 21A, SCREW CONNECTION, STANDARD SW. CAPACITY, W. TRANSVERSE AUX. SWITCH 1NO+1NC",56.28,"TEM",1,"CP",0.34399999999999997,1]
["3RV20111FA10","CIRCUIT-BREAKER SZ S00, FOR MOTOR PROTECTION, CLASS 10, A-RELEASE 3.5...5A, N-RELEASE 65A, SCREW CONNECTION, STANDARD SW. CAPACITY",45.48,"TEM",1,"CP",0.34699999999999998,1]
["3RV20111KA10","CIRCUIT-BREAKER SZ S00, FOR MOTOR PROTECTION, CLASS 10, A-RELEASE 9..12.5A, N-RELEASE 163A, SCREW CONNECTION, STANDARD SW. CAPACITY",53.93,"TEM",1,"CP",0.34399999999999997,1]
["3RV20211JA20","CIRCUIT-BREAKER SZ S0, FOR MOTOR PROTECTION, CLASS 10, A-REL. 7...10A, N-REL. 130A SPRING-L. CONNECTION, STANDARD SW. CAPACITY",53.71,"TEM",1,"CP",0.41,1]
["3RV20214EA10","CIRCUIT-BREAKER SZ S0, FOR MOTOR PROTECTION, CLASS 10, A-RELEASE 27...32A, N-RELEASE 400A, SCREW CONNECTION, STANDARD SW. CAPACITY,",89.88,"TEM",1,"CP",0.378,1]
["3RV21111GA10","CIRCUIT-BREAKER SZ S00, FOR MOTOR PROTECTION, CLASS 10, W. OVERLOAD RELAY FUNCTION A-RELEASE4.5A...6.3A, N-RELEASE82A, SCREW CONNECTION, STANDARD SW. CAPACITY",73.83,"TEM",1,"CP",0.41099999999999998,1]
["3RV23114AC20","CIRCUIT-BREAKER SZ S00, FOR STARTER COMBINATION, RATED CURRENT 16A, N-RELEASE 208A, SPRING-L. CONNECTION, STANDARD SW. CAPACITY",42.48,"TEM",1,"CP",0.375,1]
["3RV24110FA10","CIRCUIT-BREAKER SZ S00, FOR TRANSFORMER PROT. A-RELEASE 0.35...0.5A, N-RELEASE10A, SCREW CONNECTION, STANDARD SW. CAPACITY",51.04,"TEM",1,"CP",0.27300000000000002,1]
["3RV24214BA10","CIRCUIT-BREAKER SZ S0, FOR TRANSFORMER PROT. A-RELEASE 13...20A, N-RELEASE 325A, SCREW CONNECTION, STANDARD SW. CAPACITY",61.85,"TEM",1,"CP",0.35699999999999998,1]
["3RV29011E","TRANSVERSE AUX. SWITCH, 1NO+1NC, SCREW CONNECTION, FOR CIRCUIT-BREAKERS 3RV2",7.46,"TEM",1,"CP",1.7999999999999999E-2,1]
["3RV29260K","DOOR-COUPLING ROTARY MECHANISM IP64, FOR CIRCUIT-BREAKER SIZE S00...S3, BLACK, 330 MM SHAFT",40.01,"TEM",1,"CP",0.39,1]
["3RW30171BB14","SIRIUS SOFT STARTER, SIZE S00, 12.5A, 5.5KW/400V, 40 DEGREES, 200-480V AC, 110-230V AC/DC, SCREW TERMINALS",205.8,"TEM",1,"CP",0.46300000000000002,1]
["3RW30381BB04","SIRIUS SOFT STARTER, SIZE S2, 72A, 37KW/400V, 40 DEGREES, 200-480V AC, 24V AC/DC, SCREW TERMINALS",800.4,"TEM",1,"CP",1.18,1]
["3RW40261BB15","SIRIUS SOFT STARTER, S0, 25A, 15KW/500V, 40 DEGR., AC 400-600V, AC/DC 110-230V, SCREW TERMINALS",516.01,"TEM",1,"CP",0.72499999999999998,1]
["3RW40371BB04","SIRIUS SOFT STARTER, S2, 63A, 30KW/400V, 40 DEGR., AC 200-480V, AC/DC 24V, SCREW TERMINALS",904.56,"TEM",1,"CP",1.3,1]
["3RW40471BB04","SIRIUS SOFT STARTER, S3, 106A, 55KW/400V, 40 DEGR., AC 200-480V, AC/DC 24V, SCREW TERMINALS",1289.97,"TEM",1,"CP",1.885,1]
["3RW40746BB34","SIRIUS SOFT STARTER, S12, 248 A, 200 HP/460 V, 50 DEG., 200-460 V AC, 115 V AC, SCREW TERMINALS",2144.7399999999998,"TEM",1,"CP",8.9,1]
["3RW44261BC44","SIRIUS SOFT STARTER, VALUES WITH 400 V, 40 DEG., STANDARD: 77A, 37KW, INSIDE-DELTA CIRCUIT 3: 133A, 75KW, 200-460 V AC, 230 V AC, SCREW TERMINALS",1718.31,"TEM",1,"CP",5.5940000000000003,1]
["3RW44446BC34","SIRIUS SOFT STARTER, VALUES WITH 460 V, 50 DEG., STANDARD: 215A, 150HP, INSIDE-DELTA CIRCUIT 3: 372A, 300HP, 200-460 V AC, 115 V AC, SCREW TERMINALS",3928.83,"TEM",1,"CP",11.34,1]
["3RW49000AC00","EXTERNAL DISPLAY AND OPERATING MODULE F. SIRIUS SOFT STARTERS 3RW44 CONNECTING CABLE E.G. 2.5M (3UF7933-0BA00-0) NOT INCL. IN SCOPE OF SUPPPLY REQUIERD SOFTWARE VERSION 3RW44 >= *E05*. IMPLEMENTED FOR 3RW44 STARTERS FROM DELIVERY DATE 05.2006 ONWARDS",321.75,"TEM",1,"CP",0.105,1]
["3RX90200AA00","AS-I CABLE, TRAPEZOIDAL, F. EXTERNAL AUXILIARY VOLTAGE, UP TO 24V, BLACK, RUBBER, 2X 1.5QMM CONSISTS OF 100 M CABLE",364.59,"TEM",1,"CP",7.149,1]
["3SB19012EU","INSCRIPTION LABEL FOR GLUING ONTO LABEL HOLDER, LABEL SIZE 12.5 X 27MM, SILVER-COLORED, BLACK LETTERING, WITH INSCRIPTION: MAN AUTO WITH INSCRIPTION: MAN AUTO SILVER-COLORED, BLACK LETTERING",0.77,"TEM",100,"CP",1E-3,10]
["3SB19014QB","INSCRIPTION PLATE FOR ILLUMINATED PUSHBUTTON AND SWITCH, FLAT, ROUND MILKY WITH BLACK LETTERING, WITH SYMBOL: CLAMP",0.77,"TEM",100,"CP",1E-3,10]
["3SB19022BG","DRILLING TEMPLATE FOR 30 MM X 30MM GRID, HORIZONTAL AND VERTICAL SPACING, RATED CONDITION SEE INSTALLATION DIMENSIONS IN OPERATING INSTRUCTIONS",3.18,"TEM",1,"CP",2.1000000000000001E-2,1]
["3SB20010AE01","ILLUMINATED PUSHBUTTON, 16MM, ROUND, PLASTIC, GREEN, BUTTON, FLAT",5.92,"TEM",1,"CP",0.01,1]
["3SB22031AC01","EMERGENCY-STOP MUSHROOM PUSHBUTTON, 16MM, ROUND, PLASTIC, RED, LATCHING, ROTATE-TO-UNLATCH MECHANISM, 1NC, WITH YELLOW BACKING PLATE, INSCRIPTION EMERGENCY-STOP",26.55,"TEM",1,"CP",2.7E-2,1]
["3SB22246BE06","INDICATOR LIGHT, 16MM, ROUND, PLASTIC, GREEN, LAMPHOLDER W2 X 4.6D, WITH INCANDESCENT LAMP 24V",9.49,"TEM",1,"CP",0.02,1]
["3SB29080AA","HOLDER FOR SWITCHING ELEMENTS, PLUG-TYPE TERMINAL",2.87,"TEM",1,"CP",8.0000000000000002E-3,5]
["3SB30000AA41","22MM PLASTIC ROUND ACTUATOR: PUSHBUTTON WITH FLAT BUTTON WITH HOLDER GREEN",5.61,"TEM",1,"CP",2.5000000000000001E-2,1]
["3SB30001EA11","22MM PLASTIC ROUND ACTUATOR: PUSH-PULL BUTTON 30MM LATCHING W.PULL-TO-UNLOCK MECH. WITH HOLDER BLACK",15.81,"TEM",1,"CP",3.2000000000000001E-2,1]
["3SB30002DA41","22MM PLASTIC ROUND ACTUATOR: SELECTOR SWITCH 3 SWITCH POSITIONS I-O-II LATCHING NON-ILLUMINATED WITH HOLDER GREEN",9.3800000000000008,"TEM",1,"CP",2.9000000000000001E-2,1]
["3SB30003AH01","22MM PLASTIC ROUND ACTUATOR: OMR KEY-OPER.SWITCH  W. 2 KEYS 2 SWITCH POSITIONS O-I LATCHING LOCK NO 73037, REMOVAL POS. O WITH HOLDER RED",30.5,"TEM",1,"CP",0.127,1]
["3SB30004LD11","22MM PLASTIC ROUND ACTUATOR: CES KEY-OPER.SWITCH WITH 2 KEYS 2 SWITCH POSITIONS O-I LATCHING LOCK NO SSG 10, REM. POS. O+I WITH HOLDER",42.64,"TEM",1,"CP",0.14099999999999999,1]
["3SB30010BA71","22MM PLASTIC ROUND ACTUATOR: ILLUMINATED PUSHBUTTON WITH RAISED BUTTON ILLUMINABLE INCL. HOLDER FOR 3 ELEMENTS WITH HOLDER CLEAR",7.14,"TEM",1,"CP",2.5999999999999999E-2,1]
["3SB30012EA41","22MM PLASTIC ROUND ACTUATOR: SELECTOR SWITCH MOMENTARY CONTACT TYPE 3 SWITCH POSITIONS I-O-II ILLUMINATED INCL. HOLDER FOR 3 ELEMENTS WITH HOLDER GREEN",10.4,"TEM",1,"CP",0.03,1]
["3SB30016AA40","22MM PLASTIC ROUND INDICATOR: INDICATOR LIGHT WITH SMOOTH LENSE ILLUMINABLE WITH HOLDER GREEN",4.49,"TEM",1,"CP",2.3E-2,1]
["3SB32010AA51","22MM PLASTIC ROUND COMPLETE UNIT COMBINATION: PUSHBUTTON WITH FLAT BUTTON SCREW TERMINAL, 1NO+1NC WITH HOLDER BLUE",10.81,"TEM",1,"CP",4.8000000000000001E-2,1]
["3SB32010AA61","22MM PLASTIC ROUND COMPLETE UNIT COMBINATION: PUSHBUTTON WITH FLAT BUTTON SCREW TERMINAL, 1NO+1NC WITH HOLDER WHITE",10.81,"TEM",1,"CP",4.7E-2,1]
["3SB32022KA110CC0","22MM PLASTIC ROUND COMPLETE UNIT COMBINATION: SELECTOR SWITCH LATCHING 2 SWITCH POSITIONS O-I NON-ILLUMINATED SPRING-LOADED TERMINAL, 1NO WITH HOLDER BLACK",13.57,"TEM",1,"CP",4.1000000000000002E-2,1]
["3SB32050AA210CC0","22MM PLASTIC ROUND COMPLETE UNIT COMBINATION: ILLUMINATED PUSHBUTTON WITH FLAT BUTTON NON-ILLUMINATED WITH LAMP HOLDER BA 9S WITHOUT LAMP SPRING-LOADED TERMINAL, 1NO+1NC WITH HOLDER RED",17.34,"TEM",1,"CP",5.3999999999999999E-2,1]
["3SB32102DA11","22MM PLASTIC ROUND COMPLETE UNIT COMBINATION: SELECTOR SWITCH LATCHING 3 SWITCH POSITIONS I-O-II NON-ILLUMINATED SCREW TERMINAL, 1NO, 1NO WITH HOLDER BLACK",17.03,"TEM",1,"CP",5.3999999999999999E-2,1]
["3SB32337BA10","22MM PLASTIC ROUND COMPLETE UNIT COMBINATION: ACOUSTIC SIGNALING DEVICE CONTINUOUS TONE 2.4KHZ, IP65 SOUND PRESS. MIN. 80 DB./10CM, WITH LAMP HOLDER BA 9S 24V AC/DC SCREW TERMINAL WITH HOLDER BLACK",36.520000000000003,"TEM",1,"CP",4.2000000000000003E-2,1]
["3SB32446BA50","22MM PLASTIC ROUND COMPLETE UNIT COMBINATION: INDICATOR LIGHT WITH CONCENTRIC RINGS ILLUMINATED WITH INTEGRATED LED 24V AC/DC SCREW TERMINAL WITH HOLDER BLUE",10.3,"TEM",1,"CP",3.9E-2,1]
["3SB32470AA61","22MM PLASTIC ROUND COMPLETE UNIT COMBINATION: ILLUMINATED PUSHBUTTON MOMENTARY CONTACT TYPE WITH FLAT BUTTON ILLUMINATED WITH INTEGRATED LED 24V AC/DC SCREW TERMINAL, 1NO+1NC WITH HOLDER WHITE",18.36,"TEM",1,"CP",5.8000000000000003E-2,1]
["3SB32526AA60","22MM PLASTIC ROUND COMPLETE UNIT COMBINATION: INDICATOR LIGHT WITH SMOOTH LENSE ILLUMINATED WITH INTEGRATED LED 230V AC SCREW TERMINAL WITH HOLDER WHITE",14.69,"TEM",1,"CP",0.04,1]
["3SB32550AA410CC0","22MM PLASTIC ROUND COMPLETE UNIT COMBINATION: ILLUMINATED PUSHBUTTON MOMENTARY CONTACT TYPE WITH FLAT BUTTON ILLUMINATED WITH INTEGRATED LED 230V AC SPRING-LOADED TERMINAL, 1NO+1NC WITH HOLDER GREEN",24.28,"TEM",1,"CP",5.8000000000000003E-2,1]
["3SB33470AA71","26X26MM PLASTIC SQUARE COMPLETE UNIT COMBINATION: ILLUMINATED PUSHBUTTON MOMENTARY CONTACT TYPE ILLUMINATED WITH INTEGRATED LED 24V AC/DC SCREW TERMINAL, 1NO+1NC WITH HOLDER CLEAR",18.36,"TEM",1,"CP",5.7000000000000002E-2,1]
["3SB34000N","ACTUATOR-/INDICATOR COMPONENT CONTACT BLOCK WITH 2 CONTACTS DUST-RESISTANT, INCL.  LABEL SCREW TERMINAL, 1NO+1NC LABEL 3SB3901-0CH",7.04,"TEM",1,"CP",1.7999999999999999E-2,1]
["3SB34001RD","ACTUATOR-/INDICATOR COMPONENT WITH INTEGRATED LED 230V AC LAMP HOLDER SCREW TERMINAL BLUE",10.81,"TEM",1,"CP",1.0999999999999999E-2,1]
["3SB34030A","ACTUATOR-/INDICATOR COMPONENT CONTACT BLOCK WITH 2 CONTACTS SPRING-LOADED TERMINAL, 1NO+1NC FOR MOUNTING ON FRONT PLATE",7.14,"TEM",1,"CP",6.0000000000000001E-3,1]
["3SB34200C","COMPONENT FOR ENCLOSURE, 22MM CONTACT BLOCK WITH 1 CONTACT ELEMENT SCREW TERMINAL, 1NC",4.9000000000000004,"TEM",1,"CP",1.2999999999999999E-2,1]
["3SB35000AA21","22MM METAL ROUND ACTUATOR: PUSHBUTTON WITH FLAT BUTTON WITH HOLDER RED",6.15,"TEM",1,"CP",7.0000000000000007E-2,1]
["3SB35002LA11","22MM METAL ROUND ACTUATOR: SELECTOR SWITCH MOMENTARY CONTACT TYPE 2 SWITCH POSITIONS O-I NON-ILLUMINATED WITH HOLDER BLACK",10.15,"TEM",1,"CP",7.4999999999999997E-2,1]
["3SB35002LA41","22MM METAL ROUND ACTUATOR: SELECTOR SWITCH MOMENTARY CONTACT TYPE 2 SWITCH POSITIONS O-I NON-ILLUMINATED WITH HOLDER GREEN",10.15,"TEM",1,"CP",7.4999999999999997E-2,1]
["3SB35010DA41","22MM METAL ROUND ACTUATOR: ILLUMINATED PUSHBUTTON LATCHING, UNLOCKING BY PRESSING AGAIN WITH FLAT BUTTON ILLUMINABLE INCL. HOLDER FOR 3 ELEMENTS WITH HOLDER GREEN",11.07,"TEM",1,"CP",7.4999999999999997E-2,1]
["3SB35012KA41","22MM METAL ROUND ACTUATOR: SELECTOR SWITCH LATCHING 2 SWITCH POSITIONS O-I ILLUMINATED WITH HOLDER GREEN",11.38,"TEM",1,"CP",7.5999999999999998E-2,1]
["3SB36012PA11","22MM METAL ROUND COMPLETE UNIT COMBINATION: SELECTOR SWITCH HEAVY DUTY LATCHING 2 SWITCH POSITIONS O-I NON-ILLUMINATED SCREW TERMINAL, 1NO+1NC WITH HOLDER BLACK SOLVENT-RESISTANT",19.579999999999998,"TEM",1,"CP",0.12,1]
["3SB36031HA20","22MM METAL ROUND COMPLETE UNIT COMBINATION: EMERGEN.-STOP MUSHR.PUSHB. 40MM LATCH.W. ROT.-TO-UNLATCH MECH. WITH YELLOW BACKING PLATE SCREW TERMINAL, 1NC WITH HOLDER RED INSCRIPTION: NOT-HALT",22.24,"TEM",1,"CP",0.128,1]
["3SB36446BA30","INDICATOR LIGHT, 22MM, ROUND, METAL, YELLOW, LENS, CONCENTRIC RINGS, WITH HOLDER, LAMPHOLDER, WITH INTEGRATED LED AC/DC 24V, SCREW CONNECTION",10.87,"TEM",1,"CP",7.4999999999999997E-2,1]
["3SB36470AA31","22MM METAL ROUND COMPLETE UNIT COMBINATION: ILLUMINATED PUSHBUTTON MOMENTARY CONTACT TYPE WITH FLAT BUTTON ILLUMINATED WITH INTEGRATED LED 24V AC/DC SCREW TERMINAL, 1NO+1NC WITH HOLDER YELLOW",19.170000000000002,"TEM",1,"CP",0.10100000000000001,1]
["3SB36540AA21","22MM METAL ROUND COMPLETE UNIT COMBINATION: ILLUMINATED PUSHBUTTON MOMENTARY CONTACT TYPE WITH FLAT BUTTON ILLUMINATED WITH INTEGRATED LED 230V AC SCREW TERMINAL, 1NC WITH HOLDER RED",21.53,"TEM",1,"CP",9.5000000000000001E-2,1]
["3SB38012DG3","ENCLOSURE FOR COMMAND DEVICES, 22MM, ROUND, ENCLOSURE MATERIAL METAL, ENCLOSURE TOP PART YELLOW, 1 COMMAND POSITION, A=EMERG. STOP MUSHR. PUSHBUTTON RED, 40MM, ROTATE-TO-UNLATCH, 1NC, SCREW CONNECTION, FLOOR MOUNTING, 1 X M20 EACH AT TOP AND BOTTOM",52.69,"TEM",1,"CP",0.58199999999999996,1]
["3SB38032DA3","ENCLOSURE FOR 22MM PROGRAM METAL VERSION 3 COMMAND POSITIONS GRAY TOP PART A=PUSHBUTTON RED, LABEL \"O\" 1NC B=PUSHBUTTON GREEN, LABEL \"I\" 1NO C=INDICATOR LIGHT CLEAR BA9S",71.75,"TEM",1,"CP",0.86,1]
["3SB39010CK","ACCESSORY FOR ENCLOSURE, 22MM CABLE GLAND M20 WITH NUT",5.84,"TEM",1,"CP",1.7999999999999999E-2,1]
["3SB39011PA","ACCESSORY / SPARE PART ROUND, 22MM/SQUARE, 26X26MM: LED SUPER-BRIGHT LAMPS, BASE BA 9S BULB DIAMETER 10MM RATED VOLTAGE 24V AC/DC OPERATIONAL CURRENT MAX. 15 MA BLUE",6.97,"TEM",1,"CP",2E-3,10]
["3SB39021MF","INSCRIPTION ACTUATOR/INDICATOR ON LABEL HOLDER INSCRIPTION LABEL FOR STICKING = BACKING PLATE LABEL SIZE 12.5 X 27 MM WITH GRAPHICAL SYMBOL: O  I BLACK WITH WHITE PRINT",0.56999999999999995,"TEM",100,"CP",2E-3,10]
["3SB39061MF","INSCRIPTION FOR ENCLOSURE INSCRIPTION LABEL FOR STICKING LABEL SIZE 22 X 22 MM WITH GRAPHICAL SYMBOL: O  I BLACK WITH WHITE PRINT",1.44,"TEM",1,"CP",1E-3,10]
["3SB39210AU","ACCESSORY / SPARE PART FOR THE PLASTIC PROGRAM ROUND, 22MM: SINGLE FRAME FOR SQUARE DESIGN BLACK",1.54,"TEM",1,"CP",2E-3,1]
["3SB39300CA6","ACCESSORY / SPARE PART ROUND, 22MM: FLAT BUTTON FOR ILLUMIN. PUSHBUTTON AND-SWITCH WHITE",0.56999999999999995,"TEM",100,"CP",1E-3,10]
["3SE50000AA51","LENGTH-ADJUSTABLE TWIST LEVER FOR POSITION SWITCH 3SE51/52 METAL LEVER 100MM LONG STAINLESS STEEL ROLLER 19MM",14.04,"TEM",1,"CP",3.5999999999999997E-2,1]
["3SE50000AE01","ACTUATOR HEAD FOR POSITION SWITCH 3SE51 ROLLER LEVER , METAL LEVER AND PLASTIC ROLLER 22MM",14.35,"TEM",1,"CP",2.5000000000000001E-2,1]
["3SE50000AV02","SEPARATE ACTUATOR VERTICAL MOUNTING FOR POS. W. TUMBLER 3SE5312../3SE5322.. AND ASI 3SF13... AND POS. WITH SEPARATE ACTUATOR 3SE51../3SE52.. AND ASI 3SF11../3SF21..",5.54,"TEM",1,"CP",6.3E-2,1]
["3SE51120CA001CA0","BASIC SWITCH W. INCREASED CORROSION PROTECTION FOR POSITION SWITCH METAL ENCLOSURE, TO EN50041 DEVICE CONNECTION 1X (M20X1.5) 1NO/1NC SNAP-ACTION CONTACTS W/O ACTUATOR HEAD",28.09,"TEM",1,"CP",0.30399999999999999,1]
["3SE51120LA00","BASIC SWITCH FOR POSITION SWITCH 3SE51, METAL ENCLOSURE, ACC. TO EN50041 DEVICE CONNECTION 1X (M20X1.5) 1NO/2NC SNAP-ACTION CONTACTS W/O ACTUATOR HEAD",26.65,"TEM",1,"CP",0.307,1]
["3SE51220KA00","BASIC SWITCH FOR POSITION SWITCH 3SE51, METAL ENCLOSURE 56MM, TO EN50041 3X(M20X1.5) 1NO/ 2NC SLOW-ACTION CONTACTS W/O ACTUATOR HEAD",27.68,"TEM",1,"CP",0.35799999999999998,1]
["3SE51320QV20","SIRIUS POSITION SWITCH W. SEPARATE ACTUATOR,PLASTIC ENCLOSURE,40MM; 1X(M20X1.5) SLOW-ACTION CONTACTS 1NO+2NC, 5 DIRECTIONS OF APPROACH, THE MATCHING SEPARATE ACTUATOR 3SE5000-0AV0. MUST BE ORDERED SEPARATELY",38.54,"TEM",1,"CP",0.17499999999999999,1]
["3SE52320HD10","SIRIUS POSITION SWITCH PLASTIC HOUSING ACC. TO EN50047, 31MM DEVICE CONNECTION 1X(M20X1.5); 1NO/1NC SNAP-ACTION CONTACTS INTEGRATED (NOT REPLACEABLE) ROLLER PLUNGER W. CENTRAL FIXING AND PLASTIC ROLLER 10MM",25.83,"TEM",1,"CP",9.8000000000000004E-2,1]
["3SE52340KC051AE0","SIRIUS POSITION SWITCH; PLASTIC HOUSING ACC. TO EN50047, 31MM 1NO/2NC SLOW-ACTION CONTACTS W. M12 CONNECTOR,4-POLE MAX.250V AND 4A, 2OE AND PE CONNECTED TEFLON PLUNGER",31.37,"TEM",1,"CP",7.6999999999999999E-2,1]
["3SE52500PC05","SIRIUS POSITION SWITCH; PLASTIC HOUSING NOT ENCAPSULATED 30MM 2NO/1NC SLOW-ACTION CONTACTS METAL PLUNGER, IP10",18.04,"TEM",1,"CP",0.06,1]
["3SE54230CN201EA2","COMPACT SWITCH 40MM WIDE W. CONNECTING CABLE 2M SNAP-ACTION CONTACTS 1NO+1NC TWIST LEVER,",52.16,"TEM",1,"CP",0.35299999999999998,1]
["3SE67142CA","SOLENOID, RECTANGULAR LARGE 25 X 88 MM FOR MAGN.-OP. SWITCH 3SE66.7-2CA.., ACTUATOR AND SENSOR ON A FASTENING PLANE",15.89,"TEM",1,"CP",1E-3,1]
["3SE71601BD00","SIRIUS CABLE-OPER.SWITCH+LEVER METAL ENCLOSURE, 2XM25X1.5 1NO+1NC, LATCHING EN ISO 13850 AND BUTTON RESET, ACTUATION ON BOTH SIDES FOR ROPE LENGTHS UP TO 2X75M",390.12,"TEM",1,"CP",0.88900000000000001,1]
["3SE79411AB","ROPE CLAMP  3 MM",7.38,"TEM",1,"CP",1.7999999999999999E-2,1]
["3SK11211AB40","SIRIUS SAFETY RELAY BASIC UNIT ADVANCED SERIES RELAY ENABLING CIRCUITS 3 NO CONTACTS + RELAY SIGNALING CIRCUIT 1 NC CONTACT US = 24 V DC SCREW TERMINAL",215.35,"TEM",1,"CP",0.28199999999999997,1]
["3SU10000BB600AA0","PUSHBUTTON, 22MM, ROUND, PLASTIC, WHITE, RAISED BUTTON, MOMENTARY CONTACT TYPE",4.82,"TEM",1,"CP",1.9E-2,1]
["3SU10001BD400AA0","MUSHROOM PUSHBUTTON, 22MM, ROUND, PLASTIC, GREEN, 40MM, MOMENTARY CONTACT TYPE",7.28,"TEM",1,"CP",2.7E-2,1]
["3SU10004BL110AA0","RONIS KEY-OPERATED SWITCH, 22MM, ROUND, PLASTIC, LOCK NO. SB30, WITH 2 KEYS, 3 SWITCH POSITIONS I-O-II, LATCHING, ACTUATING ANGLE 2X45 DEG., 10:30H/12H/13:30H, KEY REMOVAL POS. I+O+II, POSSIBLE SPECIAL LOCKS: SB31, 421, 455",17.63,"TEM",1,"CP",5.2999999999999999E-2,1]
["3SU10011AD200AA0","ILLUM. MUSHROOM PUSHBUTTON, 22MM, ROUND, PLASTIC, RED, 30MM, MOMENTARY CONTACT TYPE",7.28,"TEM",1,"CP",2.4E-2,1]
["3SU10013AB660AL0","ILLUMINATED TWIN PUSHBUTTON, 22MM, ROUND, PLASTIC, WHITE: -, WHITE: +, FLAT BUTTONS",7.48,"TEM",1,"CP",2.1000000000000001E-2,1]
["3SU10022BF200AA0","SELECTOR SWITCH, CAN BE ILLUM., 22MM, ROUND, PLASTIC, RED, SHORT SELECTOR SWITCH, 2 SWITCH POSITIONS O-I, LATCHING, ACTUATING ANGLE 90 DEG., 10:30H/13:30H",6.77,"TEM",1,"CP",2.3E-2,1]
["3SU10022BN600AA0","SELECTOR SWITCH, CAN BE ILLUM., 22MM, ROUND, PLASTIC, WHITE, SHORT SELECTOR SWITCH, 3 SWITCH POSITIONS I-O<II, LATCHING TO THE LEFT, MOM. CONTACT TYPE TO THE RIGHT, ACTUATING ANGLE 2X45 DEG., 10:30H/12H/13:30H",6.87,"TEM",1,"CP",2.1999999999999999E-2,1]
["3SU10300AB200AD0","PUSHBUTTON, 22MM, ROUND, PLASTIC WITH METAL FRONT RING, RED, INSCRIPTION: O, FLAT BUTTON MOMENTARY CONTACT TYPE",4.51,"TEM",1,"CP",2.8000000000000001E-2,1]
["3SU10301AA200AA0","MUSHROOM PUSHBUTTON, 22MM, ROUND, PLASTIC WITH METAL FRONT RING, RED, 30MM, LATCHING, PULL TO UNLATCH",13.02,"TEM",1,"CP",3.9E-2,1]
["3SU10303BB420AK0","TWIN PUSHBUTTON, 22MM, ROUND, PLASTIC WITH METAL FRONT RING, GREEN: I, RED: O, FLAT AND RAISED BUTTONS",7.89,"TEM",1,"CP",4.2999999999999997E-2,1]
["3SU10310AA600AA0","ILLUMINATED PUSHBUTTON, 22MM, ROUND, PLASTIC WITH METAL FRONT RING, WHITE, FLAT BUTTON, LATCHING, PUSH TO UNLATCH",7.89,"TEM",1,"CP",2.5000000000000001E-2,1]
["3SU10313AB420AA0","ILLUMINATED TWIN PUSHBUTTON, 22MM, ROUND, PLASTIC WITH METAL FRONT RING, GREEN, RED, FLAT BUTTONS",8.1999999999999993,"TEM",1,"CP",4.2999999999999997E-2,1]
["3SU10322BF500AA0","SELECTOR SWITCH, CAN BE ILLUM., 22MM, ROUND, PLASTIC WITH METAL FRONT RING, BLUE, SHORT SELECTOR SWITCH, 2 SWITCH POSITIONS O-I, LATCHING, ACTUATING ANGLE 90 DEG., 10:30H/13:30H",7.18,"TEM",1,"CP",3.6999999999999998E-2,1]
["3SU10322BP200AA0","SELECTOR SWITCH, CAN BE ILLUM., 22MM, ROUND, PLASTIC WITH METAL FRONT RING, RED, SHORT SELECTOR SWITCH, 3 SWITCH POSITIONS I>O-II, MOM. CONTACT TYPE TO THE LEFT, LATCHING TO THE RIGHT, ACTUATING ANGLE 2X45 DEG., 10:30H/12H/13:30H",7.28,"TEM",1,"CP",3.5999999999999997E-2,1]
["3SU10500AB400AC0","PUSHBUTTON, 22MM, ROUND, METAL, SHINY, GREEN, INSCRIPTION: I, FLAT BUTTON MOMENTARY CONTACT TYPE",4.82,"TEM",1,"CP",0.04,1]
["3SU10501AA100AA0","MUSHROOM PUSHBUTTON, 22MM, ROUND, METAL, SHINY, BLACK, 30MM, LATCHING, PULL TO UNLATCH",13.43,"TEM",1,"CP",5.8999999999999997E-2,1]
["3SU10503AB610AK0","TWIN PUSHBUTTON, 22MM, ROUND, METAL, SHINY, WHITE: I, BLACK: O, FLAT BUTTONS",8.61,"TEM",1,"CP",7.1999999999999995E-2,1]
["3SU10511BD300AA0","ILLUM. MUSHROOM PUSHBUTTON, 22MM, ROUND, METAL, SHINY, YELLOW, 40MM, MOMENTARY CONTACT TYPE",8,"TEM",1,"CP",4.8000000000000001E-2,1]
["3SU10522BC200AA0","SELECTOR SWITCH, CAN BE ILLUM., 22MM, ROUND, METAL, SHINY, RED, SHORT SELECTOR SWITCH, 2 SWITCH POSITIONS O<I, MOMENTARY CONTACT TYPE, ACTUATING ANGLE 45 DEG., 10:30H/12H",7.59,"TEM",1,"CP",5.0999999999999997E-2,1]
["3SU10522BP600AA0","SELECTOR SWITCH, CAN BE ILLUM., 22MM, ROUND, METAL, SHINY, WHITE, SHORT SELECTOR SWITCH, 3 SWITCH POSITIONS I>O-II, MOM. CONTACT TYPE TO THE LEFT, LATCHING TO THE RIGHT, ACTUATING ANGLE 2X45 DEG., 10:30H/12H/13:30H",7.69,"TEM",1,"CP",5.0999999999999997E-2,1]
["3SU10600JB400AA0","PUSHBUTTON, 30MM, ROUND, METAL, MATT, GREEN, FRONT RING FOR FLAT INSTALL., MOMENTARY CONTACT TYPE",9.1199999999999992,"TEM",1,"CP",7.5999999999999998E-2,1]
["3SU10610JB700AA0","ILLUMINATED PUSHBUTTON, 30MM, ROUND, METAL, MATT, CLEAR, FRONT RING FOR FLAT INSTALL., MOMENTARY CONTACT TYPE",10.76,"TEM",1,"CP",7.4999999999999997E-2,1]
["3SU10622EF400AA0","SELECTOR SWITCH, CAN BE ILLUM., 30MM, ROUND, METAL, MATT, GREEN, LONG SELECTOR SWITCH, FRONT RING FOR FLAT INSTALL., 2 SWITCH POSITIONS O-I, LATCHING, ACTUATING ANGLE 90 DEG., 10:30H/13:30H",12.4,"TEM",1,"CP",8.5000000000000006E-2,1]
["3SU11002BF601BA0","SELECTOR SWITCH, CAN BE ILLUM., 22MM, ROUND, PLASTIC, BLACK, WHITE, SHORT SELECTOR SWITCH, 2 SWITCH POSITIONS O-I, LATCHING, 10:30H/13:30H, WITH HOLDER, 1NO, SCREW TERMINAL",11.28,"TEM",1,"CP",5.8000000000000003E-2,1]
["3SU11030AB501BA0","ILLUMINATED PUSHBUTTON, 22MM, ROUND, PLASTIC, BLUE, FLAT BUTTON, MOMENTARY CONTACT TYPE, WITH HOLDER, 1NO, LED MODULE, WITH INTEGRATED LED 110V AC, SCREW TERMINAL",17.63,"TEM",1,"CP",5.8000000000000003E-2,1]
["3SU11066AA203AA0","INDICATOR LIGHT, 22MM, ROUND, PLASTIC, RED, SMOOTH LENS, WITH HOLDER, LED MODULE, WITH INTEGRATED LED 230V AC, SPRING-TYPE TERMINAL",13.74,"TEM",1,"CP",4.2999999999999997E-2,1]
["3SU11304BL111NA0","RONIS KEY-OPERATED SWITCH, 22MM, ROUND, PLASTIC WITH METAL FRONT RING, LOCK NO. SB30, WITH 2 KEYS, 3 SWITCH POSITIONS I-O-II, LATCHING, ACTUATING ANGLE 2X45 DEG., 10:30H/12H/13:30H, KEY REMOVAL POS. I+O+II, WITH HOLDER, 1NO, 1NO, SCREW TERMINAL",26.34,"TEM",1,"CP",0.1,1]
["3SU11500AB201BA0","PUSHBUTTON, 22MM, ROUND, METAL, SHINY, RED, FLAT BUTTON, MOMENTARY CONTACT TYPE, WITH HOLDER, 1NO, SCREW TERMINAL",8.82,"TEM",1,"CP",9.1999999999999998E-2,1]
["3SU11520AB201CA0","ILLUMINATED PUSHBUTTON, 22MM, ROUND, METAL, SHINY, RED, FLAT BUTTON, MOMENTARY CONTACT TYPE, WITH HOLDER, 1NC, LED MODULE, WITH INTEGRATED LED 24V AC/DC, SCREW TERMINAL",14.56,"TEM",1,"CP",9.9000000000000005E-2,1]
["3SU11536AA301AA0","INDICATOR LIGHT, 22MM, ROUND, METAL, SHINY, YELLOW, SMOOTH LENS, WITH HOLDER, LED MODULE, WITH INTEGRATED LED 110V AC, SCREW TERMINAL",13.12,"TEM",1,"CP",8.2000000000000003E-2,1]
["3SU12002PQ101AA0","POTENTIOMETER, COMPACT, 22MM, ROUND, PLASTIC, BLACK, 1K OHMS, WITH HOLDER, SCREW TERMINALS",27.78,"TEM",1,"CP",6.5000000000000002E-2,1]
["3SU14011BH401AA0","LED MODULE WITH INTEGRATED LED, 24-240V AC/DC, GREEN, SCREW TERMINAL, FOR FRONT PLATE MOUNTING",10.56,"TEM",1,"CP",1.0999999999999999E-2,1]
["3SU14011BH403AA0","LED MODULE WITH INTEGRATED LED, 24-240V AC/DC, GREEN, SPRING-TYPE TERMINAL, FOR FRONT PLATE MOUNTING",11.58,"TEM",1,"CP",0.01,1]
["3SU15500AA100AA0","HOLDER FOR 3 MODULES, METAL",1.44,"TEM",1,"CP",4.3999999999999997E-2,1]
["3SU18510AB002AB1","ENCLOSURE FOR COMMAND DEVICES, 22MM, ROUND, ENCLOSURE MATERIAL METAL, ENCLOSURE TOP PART GRAY, 1 COMMAND POINT METAL, A=PUSHBUTTON GREEN, 1NO, SCREW TERMINAL, BASE MOUNTING, LABEL: I, TOP AND BOTTOM 1 X M20 EACH",30.44,"TEM",1,"CP",0.56799999999999995,1]
["3SU19000AB710QD0","INSERT LABEL FOR ILLUMINATED PUSHBUTTON, ROUND, MILKY WITH BLACK LETTERING, WITH GRAPHIC SYMBOL: III",0.63,"TEM",100,"CP",2E-3,10]
["3SU19000AC160QG0","LABELING PLATE SNAP-ON OR SELF-ADHESIVE FOR LABEL HOLDER, LABEL SIZE 12.5 X 27MM, LABEL BLACK, LETTERING WHITE, WITH GRAPHIC SYMBOL: O  I",0.49,"TEM",100,"CP",1E-3,10]
["3SU19000AN100AA0","LABEL HOLDER, FRAME WITH SQUARE BOTTOM, BLACK, FOR LABELING PLATE 12.5MM X 27MM",0.49,"TEM",100,"CP",2E-3,1]
["3SU19000FV400AA0","ID KEY ID-GROUP1, GREEN",6.15,"TEM",1,"CP",4.0000000000000001E-3,1]
["3SX3170","ACTUATORS FOR 3SE55 (3SE3200,3SE3210) POS.SW. ROLLER PLUNGER",6.11,"TEM",1,"CP",1.2E-2,1]
["3TC44170AN4","CONTACTOR SIZE 2 2-POLE DC-3 AND 5, 32 A AUXILIARY SWITCH 22 (2NO+2NC) DC OPERATION DC 250 V",261.79000000000002,"TEM",1,"CP",1.0509999999999999,1]
["3TC52170AF4","CONTACTOR, SIZE 8, 2-POLE DC-3 AND 5,RATD.OPER.CURR. 220A AUXILIARY CONTACTS 22 (2NO+2NC) DC OPERATION DC 110V",1400.05,"TEM",1,"CP",9.734,1]
["3TF20011BB4","CONTACTOR, SIZE 00, 3-POLE AC-3, 4KW/400V,PLUG-IN CONNECT. AUXILIARY CONTACT 01E (1NC) DC SOLENOID SYSTEM DC 24V",55.2,"TEM",1,"CP",0.27,1]
["3TG10010AL2","CONTACTOR SCREW TERMINALS, 3NO+1NC FOR SNAPPING ONTO STANDARD MOUNTING RAIL AC OPERATION AC 230V,45...450HZ",19.7,"TEM",1,"CP",0.158,1]
["3TG10100AC2","CONTACTOR SCREW TERMINALS, 4NO FOR SNAPPING ONTO STANDARD MOUNTING RAIL AC OPERATION AC 24V 45...450HZ",19.7,"TEM",1,"CP",0.158,1]
["3TH20220DB4","CONTACTOR RELAY 22E EN 50 011 2NO+2NC, SCREW TERMINALS DIODE OR VARISTOR PLUGGABLE DC OPERATION, COIL 2W DC 24V",48.96,"TEM",1,"CP",0.215,1]
["3TH20310BB4","CONTACTOR RELAY 31E EN 50 011 3NO+1NC, SCREW TERMINALS DC OPERATION DC SOLENOID SYSTEM DC 24V",48.33,"TEM",1,"CP",0.217,1]
["3TH42440BP4","CONTACTOR RELAY 44E EN 50 011 4NO+4NC, SCREW TERMINALS DC OPERATION DC SOLENOID SYSTEM DC 230V",113.95,"TEM",1,"CP",0.64700000000000002,1]
["3TH42440LB4","CONTACTOR RELAY 44E EN 50 011 FOR RAILWAY APPLICATIONS 4NO+4NC, SCREW TERMINAL SETTING RANGE 0.7 TO 1.25X US VARISTOR INCORPORATED DC SOLENOID SYSTEM DC 24V",120.89,"TEM",1,"CP",0.68200000000000005,1]
["3TH43550BB4","CONTACTOR RELAY 55E EN 50 011 5NO+5NC, SCREW TERMINALS DC OPERATION DC SOLENOID SYSTEM DC 24V",144.9,"TEM",1,"CP",0.70399999999999996,1]
["3TH43820BW4","CONTACTOR RELAY 82E EN 50 011 8NO+2NC, SCREW TERMINALS DC OPERATION DC SOLENOID SYSTEM DC 48V",144.9,"TEM",1,"CP",0.56599999999999995,1]
["3TK14420AP0","AC-1 CONTACTOR, 4-POLE, 550 A, MAIN CONTACTS 4 NO, AUXILIARY CONTACTS 2NO+2NC, AC OPERATION AC 220...230V 50HZ/AC 240V 60HZ",2070.9,"TEM",1,"CP",19.600000000000001,1]
["3TK19700AM7","MAGNET COIL FOR 3TK10 220...230 V AC, 40...400 HZ",111.6,"TEM",1,"CP",0.437,1]
["3TK28050BB4","CONTACTOR COMBINATION FOR SAFETY CIRCUITS ENABLING AND SIGNALLING CIRCUIT 5N0+1NC, DC OPERATION DC 24V",573.69000000000005,"TEM",1,"CP",1.06,1]
["3TK28242BB40","SIRIUS SAFETY RELAY WITH RELAY RELEASE CIRCUITS (RC), DC 24V, 22.5MM, SPRING-LOADED TERMINAL, RC INSTANT.: 2NO, RC DELAYED: 0NO, MC: 0NC, AUTOSTART, BASIC DEVICE, MAX. ACHIEVABLE SIL: 1, PL: C",166.36,"TEM",1,"CP",0.23499999999999999,1]
["3TK28271BB41","SIRIUS SAFETY RELAY WITH RELAY RELEASE CIRCUITS (RC), DC 24V, 45.0MM, SCREW TERMINAL, RC INSTANT.: 2NO, RC DELAYED: 2NO 0.05...3S, MC: 1NC, MONITORED START, BASIC DEVICE, MAX. ACHIEVABLE SIL: 3/2, PL: E/D",394.73,"TEM",1,"CP",0.45700000000000002,1]
["3TK28451GB42","SIRIUS SAFETY RELAY  WITH REL.- U. EL. RELEASE CIRCUIT (RC), DC 24V, 45.0MM, SCREW TERMINAL,  RC INSTANT.: 2S,  RC DELAYED: 1, MK: 1, SOLENOID-LOCKED TUMBLER, BASIC DEVICE, MAX. ACHIEVABLE PL TO EN13849-1: E, MAX. ACHIEVABLE SIL TO IEC61508:3,",372.28,"TEM",1,"CP",0.42,1]
["3TX44121A","AUXILIARY CONTACT BLOCK W. SCREW TERMINAL F. MOTOR CONTACTORS ACC. TO DIN EN50012 IDENTIFICAT.NUMBER 22E, 1NO+2NC",13.97,"TEM",1,"CP",4.8000000000000001E-2,1]
["3TX70021AB00","OUTPUT INTERFACE     !!! PHASE-OUT PRODUCT !!! FOR FURTHER INFORMATION PLEASE CONTACT OUR SALES STAFF! TERMINAL-TYPE COUPLING RELAY 1NO, AC/DC 24V",37.799999999999997,"TEM",1,"CP",3.1E-2,1]
["3TX70024AG00","INPUT INTERFACE     !!! PHASE-OUT PRODUCT !!! FOR FURTHER INFORMATION PLEASE CONTACT OUR SALES STAFF! TERMINAL-TYPE OPTOCOUPLER RELAY 1NO (TRANSISTOR) INPUT AC 110 TO 240V OUTPUT DC MAX. 30V",72.3,"TEM",1,"CP",3.3000000000000002E-2,1]
["3TX70043AC14","OUTPUT INTERFACE     !!! PHASE-OUT PRODUCT !!! FOR FURTHER INFORMATION PLEASE CONTACT OUR SALES STAFF! TWO-TIER TERMINAL-TYPE OPTOCOUPLERS 1N0, TRANSISTOR AC/DC 24-48V WITH MANUAL-0-AUTO SCREW TERMINAL WIDTH 12.5MM",77.400000000000006,"TEM",1,"CP",5.2999999999999999E-2,1]
["3TX74023G","SURGE SUPPRESSOR VARISTOR WITH WIRE SPACER AC 24 TO 48V/DC 24 TO 70V FOR MOUNTING TO COIL TERMINAL FOR CONTACTORS SIZE 0 TO 2",9.83,"TEM",1,"CP",1.6E-2,1]
["3TY65400A","MAIN CONTACTS F.3TB54 CONTACTOR",424.6,"TEM",1,"CP",0.53,1]
["3TY65660AF0","COIL FOR 3TC56 AC 50HZ 110V / 60HZ 132V",113.8,"TEM",1,"CP",0.63800000000000001,1]
["3TY75430AP0","COIL FOR CONTACTORS 3TF54/55 AND 3TK54 AC 230/220V 50HZ, 276/264V 60HZ",100,"TEM",1,"CP",0.53700000000000003,1]
["3TY75630AR2","COIL FOR CONTACTORS 3TF56 AND 3TK56 AC 440V 50/60HZ",124.7,"TEM",1,"CP",0.85,1]
["3UF70001AU000","BASIC UNIT 1 SIMOCODE PRO C; PROFIBUS DP-INTERFACE 12 MBIT/S, RS485; 4I/3O FREELY PARAMETERIZABLE; US: AC/DC 110-240V; THERMISTOR MOTOR PROTECTION; OUTPUTS MONOSTABLE",428.4,"TEM",1,"CP",0.32400000000000001,1]
["3UF71121AA000","CURRENT/VOLTAGE MEASUR. MODULE; SET CURRENT 10...100A; VOLTAGE DETECTION UP TO 690V; OVERALL WIDTH 55MM; STRAIGHT-THROUGH CT",260.10000000000002,"TEM",1,"CP",0.37,1]
["3UF79010AA000","MEMORY MODULE, FOR PARAMETERIZING OF SIMOCODE PRO V PN W/O  PC/PG",35.5,"TEM",1,"CP",3.0000000000000001E-3,1]
["3UG32072A","DOUBLE-POLE WIRE ELECTRODE FOR LEVEL MONITORING, 500 MM LONG, WITH TEFLON INSULATION",82.38,"TEM",1,"CP",0.23499999999999999,1]
["3UG45131BR20","ANALOG MONITORING RELAY PHASE FAILURE AND -SEQUENCE ADJUSTABLE UNDERVOLTAGE UNBALANCE 20% FIXED 3X 160 TO 690V AC 50 TO 60 HZ HYSTERESIS 5% FIXED DELAY TIME 0-20S 2 CHANGEOVER CONTACTS SCREW TERMINAL REPLACEMENT PRODUCT FOR 3UG3013-1B...",110.76,"TEM",1,"CP",0.14000000000000001,1]
["3UG46221AW30","DIGITAL MONITORING RELAY CURRENT MONITORING, 22.5MM FROM 0.05 TO 10A AC/DC OVERSHOOT A. UNDERSHOOT AC/DC 24 TO 240V DC AND AC 50 TO 60 HZ ON AND SPIKE DELAY 0.1 TO 20S HYSTERESIS 0.01 TO 5A 1 CO CONTACT W. OR W/O ERROR MEMORY SCREW CONNECTION REPLACEMENT PRODUCT FOR 3UG3522-1AL20, 3UG3522-1AG20 AND 3UG3522-1AC48-0AA1",126.29,"TEM",1,"CP",0.14599999999999999,1]
["3UG46332AL30","DIGITAL MONITORING RELAY VOLTAGE MONITORING, 22.5MM FROM 17 TO 275V AC/DC OVERSHOOT AND UNDERSHOOT INTERNAL POWER SUPPLY DC AND AC 50 TO 60 HZ SPIKE DELAY 0.1 TO 20S HYSTERESIS 0.1 TO 150V 1 CHANGEOVER CONTACT SPRING-LOADED TYPE",126.29,"TEM",1,"CP",0.13,1]
["3ZY12121BA00","DEVICE CONNECTOR FOR SAFETY RELAY 3SK1 WIDTH 17.5 MM, FOR THE ELECTR. CONNECTION OF SIRIUS DEVICES IN THE INDUSTR. DIN RAIL ENCLOSURE",15.13,"TEM",1,"CP",0.05,1]
["4AM34428JN000EA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,1 /0,31; UPRI(V):400-230+/-15; USEC(V):24; ISEC(A):4,17; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREWS/MOUNTING RAILS; EN 61558-2-2, -2-6 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >SAFETY ISOLATING TRANSFORMER<",87.54,"TEM",1,"CP",3,1]
["4AM46425AN000EA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,4 /1,44; UPRI(V):400+/-5%; USEC(V):24; ISEC(A):16,7; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-2, -2-6 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >SAFETY ISOLATING TRANSFORMER<",194.34,"TEM",1,"CP",5.76,1]
["4AM55425AT100FA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):0,8 /3,4; UPRI(V):400+/-5%; USEC(V):230; ISEC(A):3,48; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",307.5,"TEM",1,"CP",12.15,1]
["4AM65425AT100FA0","TRANSFORMER SITAS; PHASES:1; PN/PN(S6)(KVA):2,5 /13,3; UPRI(V):400+/-5%; USEC(V):230; ISEC(A):10,9; F(HZ):50...60; VECTOR GR./SHIELD WNG.:II0 /0; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW/TAB CONNECTION; INSTALLATION:SCREW; EN 61558-2-1, -2-2, -2-4 >UL/CSA-RECOGNIZED< >CONTROL CIRCUIT TRANSFORMER< >ISOLATION TRANSFORMER<",831.69,"TEM",1,"CP",31.24,1]
["4AV32002EB000A","POWER SUPPLY; PHASES:3; PN(KW):0,48; UPRI(V):400+/-20; USEC(V DC):24; ISEC(A DC):20/24 (60/40 CEL); F(HZ):50...60; VECTOR GR./SHIELD WNG.:YD1 /0; PROTECTION CL.:I; TA/ISOKL:60 /B; W(%):4,2; IP00; TYPE OF TERMINALS:SCREW CONNECTION; INSTALLATION:SCREW; EN 61558-2-6, EN61131-2 >UL/CSA-RECOGNIZED< >SAFETY ISOLATING TRANSFORMER<",490.77,"TEM",1,"CP",9.15,1]
["4EP36004US00","MAINS CHOKE F.FU; PHASES:3; UN1(V):480; ITHMAX 1(A) / F1(HZ):18 /60; I LN (A):16,2; UK(%):2; LN(MH):0,783; TA/ISOKL:40 /B; IP00; TYPE OF TERMINALS:SCREW CONNECTION; EN 61558-2-20 >UL/CSA-RECOGNIZED< >CHOKE<",287.72000000000003,"TEM",1,"CP",3.4,1]
["4EU27520UB000AA0","MAINS CHOKE F.FU; PHASES:3; UN1(V):480; ITHMAX 1(A) / F1(HZ):280 /60; I LN (A):252; UK(%):2; LN(MH):0,0503; TA/ISOKL:40 /H; IP00; TYPE OF TERMINALS:FLAT-TYPE TERMINAL; EN 61558-2-20 >UL/CSA-RECOGNIZED< >CHOKE<",1773.76,"TEM",1,"CP",28,1]
["6GK12100SA01","SIMATIC NET, REPEATER FOR AS-INTERFACE FOR  CABLE PROLONGATION IN K45 HOUSING",375.91,"TEM",1,"CP",0.122,1]
["7PV15121AQ30","TIME RELAY, ON-DELAY, 1CO, TIME RANGE 0.5 S...10 S, AC 24/110 V AND DC 24 V, WITH LED",27.88,"TEM",1,"CP",6.8000000000000005E-2,1]
["8WD42205BD","FLASHING INDICATOR ELEMENT WITH INTEG. LED, YELLOW, 24V AC/DC DIAMETER 50MM",75.17,"TEM",1,"CP",5.6000000000000001E-2,1]
["8WD43080DE","ADAPTER FOR BASE, CABLE OUTLET LATERALLY WITH MAGNET FOR MOUNTING",73.64,"TEM",1,"CP",0.30599999999999999,1]
["8WD44080AD","SIGNALLING COLUMN CONNECT. ELEMENT FOR WITH PIPE MOUNTING COVER LID, CAGE CLAMP",35.39,"TEM",1,"CP",0.104,1]
["8WD44205AF","SIGNALLING COLUMN STEADY LIGHT LED BLUE, 24V AC/DC",64.16,"TEM",1,"CP",7.2999999999999995E-2,1]
["8WD44405BD","SIGNALLING COLUMN REP.-FLASH LIGHT ELEMENT LED YELLOW, 115V AC",82.59,"TEM",1,"CP",7.3999999999999996E-2,1]
["8WD44586XB","SIGNALLING COLUMNS, ACCESSORIES LED 230V AC, BA 15D, RED",38.92,"TEM",1,"CP",1.7999999999999999E-2,1]
["LZS:PT3A5L24","PLUG-IN RELAY, COMPLETE UNIT 24 V DC, 3 CO CONTACT LED MODULE RED STANDARD PLUG-IN SOCKET SCREW TERMINAL 3.5 MM PINNING",12.73,"TEM",1,"CP",9.6000000000000002E-2,5]
["LZS:PTML0730","LED MODULE,RED FOR PLUG-IN RELAY, SERIES PT AND RT, 110..230V AC, W.OUT FREE-WHEELING DIODE",2.59,"TEM",1,"CP",2E-3,1]
["LZS:RT4B4S15","PLUG-IN RELAY COMPACT UNIT AC 115V, 2 CO CONTACT LED MODULE RED SOCKET W. LOGIC ISOLATION SCREW TERMINAL",16.04,"TEM",1,"CP",6.4000000000000001E-2,5]
["LZX:RT314024","PLUG-IN RELAY 1CO RELAY 15MM, 24V DC",3.62,"TEM",1,"CP",1.4999999999999999E-2,1]
["LZX:RT424730","PLUG-IN RELAY 2CO RELAY 15MM, 230V AC",6.93,"TEM",1,"CP",1.4999999999999999E-2,1]
["3VL17041EA460AA0","CIRCUITBREAKER VL160X N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 4 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=40A, RATED CURRENT IR=40A, OVERLOAD II=600A, SHORTCIRCUIT N PROTECTED WITH SCREW CONNECTION WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",196.13,"TEM",1,"LP",2.6589999999999998,1]
["3VL17081DA330AA0","CIRCUITBREAKER VL160X N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=80A, RATED CURRENT IR=80A, OVERLOAD II=1000A, SHORTCIRCUIT WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",154.55000000000001,"TEM",1,"LP",2.2280000000000002,1]
["3VL17162DA330AA0","CIRCUITBREAKER VL160X H HIGH BREAKING CAPACITY ICU=70KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=160A, RATED CURRENT IR=160A, OVERLOAD II=1500A, SHORTCIRCUIT WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",340.67,"TEM",1,"LP",2.23,1]
["3VL27061DC332SD1","CIRCUITBREAKER VL 160N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=63A, RATED CURRENT IR=5063A, OVERLOAD II=300600A, SHORT CIRCUIT UNDERVOLTAGE RELEASE 220  250 V DC AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO) AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO)",340.45,"TEM",1,"LP",2.2000000000000002,1]
["3VL27063DK330AA0","CIRCUITBREAKER VL 160L VERY HIGH BREAKING CAPACITY ICU=100KA / 415 V AC 3 POLE, STARTER COMBINATION PROTECTION OVERCURRENT RELEASE MAGNETIC IN=63A, RATED CURRENT II=450900A, SHORT CIRCUIT WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",364.98,"TEM",1,"LP",2.512,1]
["3VL27101DC360AB1","CIRCUITBREAKER VL 160N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=100A, RATED CURRENT IR=80100A, OVERLOAD II=5001000A, SHORT CIRCUIT WITH SCREW CONNECTION WITHOUT AUXILIARY RELEASE AUXILIARY SWITCH KIT 2HS(1NO+1NC) AUXILIARY SWITCH KIT 2HS(1NO+1NC)",256.19,"TEM",1,"LP",2.2000000000000002,1]
["3VL27102SB360AA0","CIRCUITBREAKER VL 160H HIGH BREAKING CAPACITY ICU=70KA / 415 V AC 3 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU10, LI IN=100A, RATED CURRENT IR=40100A, OVERLOAD II=1,25TO11XIN, SHORT CIRCUIT WITH SCREW CONNECTION WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",404.14,"TEM",1,"LP",2.3119999999999998,1]
["3VL27121DC360AD1","CIRCUITBREAKER VL 160N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=125A, RATED CURRENT IR=100125A, OVERLOAD II=6251250A, SHORT CIRCUIT WITH SCREW CONNECTION WITHOUT AUXILIARY RELEASE AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO)",304.58999999999997,"TEM",1,"LP",2.363,1]
["3VL27161SB330AA0","CIRCUITBREAKER VL 160N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU10, LI IN=160A, RATED CURRENT IR=64160A, OVERLOAD II=1,25TO11XIN, SHORT CIRCUIT WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",401.06,"TEM",1,"LP",2.4420000000000002,1]
["3VL27162MB330AB1","CIRCUITBREAKER VL 160H HIGH BREAKING CAPACITY ICU=70KA / 415 V AC 3 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU10, LI IN=160A, RATED CURRENT IR=64160A, OVERLOAD II=1,25TO11XIN, SHORT CIRCUIT WITHOUT AUXILIARY RELEASE ETU COMMUNICATIONCAPABLE AUXILIARY SWITCH KIT 2HS(1NO+1NC) AUXILIARY SWITCH KIT 2HS(1NO+1NC)",546.48,"TEM",1,"LP",2.4,1]
["3VL37201EJ462SD1","CIRCUITBREAKER  VL 250N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 4 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=200A, RATED CURRENT IR=160200A, OVERLOAD II=10002000A, SHORTCIRCUIT N  NOT PROTECTED UNDERVOLTAGE RELEASE 220  250 V DC AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO) AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO)",675.84,"TEM",1,"LP",3.2,1]
["3VL37251DC362HD1","CIRCUITBREAKER  VL 250N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=250A, RATED CURRENT IR=200250A, OVERLOAD II=12002500A, SHORTCIRCUIT UNDERVOLTAGE RELEASE 220  250 V AC AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO)",557.15,"TEM",1,"LP",2.774,1]
["3VL37251SE368TD1","CIRCUITBREAKER  VL 250N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU20, LSI IN=250A, RATED CURRENT IR=100250A, OVERLOAD ISD=1,5TO10XIR, II=11XIN SHORTCIRCUIT SHUNT RELEASE 208  277 V AC AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO) AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO)",665.61,"TEM",1,"LP",2.5,1]
["3VL37253DC330AA0","CIRCUITBREAKER  VL 250L VERY HIGH BREAKING CAPACITY ICU=100KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=250A, RATED CURRENT IR=200250A, OVERLOAD II=12002500A, SHORTCIRCUIT WITH BOX TERMINAL WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",662.31,"TEM",1,"LP",2.78,1]
["3VL47311TH460AA0","CIRCUITBREAKER VL 400N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 4 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU22, LSIG IN=315A, RATED CURRENT IR=128315A, OVERLOAD ISD=1,5TO10XIR, II=11XIN SHORTCIRCUIT N PROTECTED WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",1621.18,"TEM",1,"LP",7.9409999999999998,1]
["3VL47401DC362SD1","CIRCUITBREAKER VL 400N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=400A, RATED CURRENT IR=320400A, OVERLOAD II=20004000A, SHORT CIRCUIT UNDERVOLTAGE RELEASE 220  250 V DC AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO) AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO)",892.87,"TEM",1,"LP",5.7,1]
["3VL57502DK360AE1","CIRCUITBREAKER VL 630H HIGH BREAKING CAPACITY ICU=70KA / 415 V AC 3 POLE, STARTER COMBINATION PROTECTION OVERCURRENT RELEASE MAGNETIC IN=500A, RATED CURRENT II=32506300A, SHORT CIRCUIT WITHOUT AUXILIARY RELEASE AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO) AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO)",1189.43,"TEM",1,"LP",9,1]
["3VL57631EJ460AA0","CIRCUITBREAKER VL 630N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 4 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=630A, RATED CURRENT IR=500630A, OVERLOAD II=32506500A, SHORT CIRCUIT N  NOT PROTECTED WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",1341.34,"TEM",1,"LP",11.2,1]
["3VL67803SB360AE1","CIRCUITBREAKER  VL 800L VERY HIGH BREAKING CAPACITY ICU=100KA / 415 V AC 3 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU10, LI IN=800A, RATED CURRENT IR=320800A, OVERLOAD II=1,25TO8XIN, SHORTCIRCUIT WITHOUT AUXILIARY RELEASE AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO) AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO)",1984.73,"TEM",1,"LP",16,1]
["3VL87161SB308TA0","CIRCUITBREAKER VL 1600N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU10, LI IN=1600A, RATED CURRENT IR=6401600A, OVERLOAD II=1,25TO9XIN, SHORT CIRCUIT SHUNT RELEASE 208  277 V AC WITHOUT AUXILIARY/ALARM SWITCH WITHOUT AUXILIARY/ALARM SWITCH",4302.9799999999996,"TEM",1,"LP",31.3,1]
["3VL92004WA30","ACCESSORY FOR VL160, DRAW OUT ASSEMBLY REAR CONNECTORS 3 POLES",257.07,"TEM",1,"LP",4.9400000000000004,1]
["3VL93003MN00","ACCESSORY FOR VL160X, VL160, VL250, STORED ENERGY OPERATOR 110127V AC/DC",414.48,"TEM",1,"LP",2.782,1]
["3VL93258TC00","ACCESSORY FOR VL250, CURRENT TRANSFORMER FOR OVERLOAD PROTECTION OF THE NCONDUCTOR AND FOR EARTHFAULT PROTECTION IN=250A",170.61,"TEM",1,"LP",0.45500000000000002,1]
["3VL94004EC30","ACCESSORY FOR VL400, FRONT BUSBAR CONNECTION SET OF 3 PCS 3 POLE",42.79,"TEM",1,"LP",0.91800000000000004,1]
["3VL95637DC30","OVERCURRENT RELEASE VL 630 3 POLES,  LINE PROTECTION THERMAL MAGNETIC, LI IR=500630A, OVERLOAD II=32506500A, SHORT CIRCUIT",435.49,"TEM",1,"LP",1.62,1]
["3VL97158HA00","ACCESSORY FOR VL160X  VL1600, INSTALL. KIT WITH SAFETY LOCK RONIS, FOR FRONT ROTARY OPER. MECH. AND MOT. OPER. MECH. (FOR VL400  VL1600)",69.3,"TEM",1,"LP",0.26700000000000002,1]
["3VL98008BC00","ACCESSORY FOR VL1250, VL1600, COVER FRAME IP30 FOR CIRCUIT BREAKER FIXED/PLUG IN MOUNTED",21.67,"TEM",1,"LP",6.4000000000000001E-2,1]
["3VL47311DC360AB1","CIRCUITBREAKER VL 400N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=315A, RATED CURRENT IR=250315A, OVERLOAD II=15753150A, SHORT CIRCUIT WITHOUT AUXILIARY RELEASE AUXILIARY SWITCH KIT 2HS(1NO+1NC)",727.54,"TEM",1,"LP",6.2450000000000001,1]
["3VL91003ME10","ACCESSORY FOR VL160X MOTOR OPERATOR 220250 V AC/DC",283.47000000000003,"TEM",1,"LP",1.802,1]
["3VL17031DA330AB1","CIRCUITBREAKER VL160X N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=32A, RATED CURRENT IR=32A, OVERLOAD II=300A, SHORTCIRCUIT WITHOUT AUXILIARY RELEASE AUXILIARY SWITCH KIT 2HS(1NO+1NC)",190.41,"TEM",1,"LP",2.0379999999999998,1]
["3VL17051EH430AA0","CIRCUITBREAKER VL160X N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 4 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=50A, RATED CURRENT IR=50A, OVERLOAD II=600A, SHORTCIRCUIT N NOT PROTECTED WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",190.19,"TEM",1,"LP",2.9380000000000002,1]
["3VL17082DA330AA0","CIRCUITBREAKER VL160X H HIGH BREAKING CAPACITY ICU=70KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=80A, RATED CURRENT IR=80A, OVERLOAD II=1000A, SHORTCIRCUIT WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",178.97,"TEM",1,"LP",2.2349999999999999,1]
["3VL17121EH460AD1","CIRCUITBREAKER VL160X N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 4 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=125A, RATED CURRENT IR=125A, OVERLOAD II=1000A, SHORTCIRCUIT N NOT PROTECTED WITH SCREW CONNECTION WITHOUT AUXILIARY RELEASE AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO) AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO)",315.81,"TEM",1,"LP",2.5,1]
["3VL17961DA330AD1","CIRCUITBREAKER VL160X N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=16A, RATED CURRENT IR=16A, OVERLOAD II=300A, SHORTCIRCUIT WITHOUT AUXILIARY RELEASE AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO) AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO)",204.6,"TEM",1,"LP",1.9,1]
["3VL27081EJ430AA0","CIRCUITBREAKER VL 160N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 4 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=80A, RATED CURRENT IR=6380A, OVERLOAD II=400800A, SHORT CIRCUIT N  NOT PROTECTED WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",272.25,"TEM",1,"LP",3.1150000000000002,1]
["3VL27101EM430AD1","CIRCUITBREAKER VL 160N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 4 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=100A, RATED CURRENT IR=80100A, OVERLOAD II=5001000A, SHORT CIRCUIT N  PROTECTED WITHOUT AUXILIARY RELEASE AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO) AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO)",349.47,"TEM",1,"LP",3,1]
["3VL27121DC330AA0","CIRCUITBREAKER VL 160N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=125A, RATED CURRENT IR=100125A, OVERLOAD II=6251250A, SHORT CIRCUIT WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",256.63,"TEM",1,"LP",2.4260000000000002,1]
["3VL27161DC368TB1","CIRCUITBREAKER VL 160N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=160A, RATED CURRENT IR=125160A, OVERLOAD II=8001600A, SHORT CIRCUIT WITH SCREW CONNECTION SHUNT RELEASE 208  277 V AC AUXILIARY SWITCH KIT 2HS(1NO+1NC) AUXILIARY SWITCH KIT 2HS(1NO+1NC)",435.71,"TEM",1,"LP",2.2000000000000002,1]
["3VL27161SS330AA0","CIRCUITBREAKER VL 160N STANDARD BREAKING CAPACITY R.U.S.C.BR.C.= 55KA, 415 V AC 3POLE, MOTOR PROTECTION ELECTRONIC TRIP UNIT ETU30M, LI IN=160A, RATED CURRENT TC= 10A ... 30, TIME LAG CLASS II= 6 ... 11 X IN, SHORTCIRCUIT PROTECTION WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",405.13,"TEM",1,"LP",2.4300000000000002,1]
["3VL27162SP360AD1","CIRCUITBREAKER VL 160H HIGH BREAKING CAPACITY ICU=70KA / 415 V AC 3 POLE, MOTOR/ GENERATOR PROTECTION ELECTRONIC TRIP UNIT ETU10M, LI IN=160A, RATED CURRENT IR=64160A, OVERLOAD II=1,25TO11XIN,  SHORT CIRCUIT WITH SCREW CONNECTION WITHOUT AUXILIARY RELEASE AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO) AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO)",484.22,"TEM",1,"LP",2.4,1]
["3VL37201SS360AD1","CIRCUITBREAKER VL 250N STANDARD BREAKING CAPACITY R.U.S.C.BR.C.= 55KA, 415 V AC 3POLE, MOTOR PROTECTION ELECTRONIC TRIP UNIT ETU30M, LI IN=200A, RATED CURRENT TC= 10A ... 30, TIME LAG CLASS II= 6 ... 11 X IN, SHORTCIRCUIT PROTECTION WITHOUT AUXILIARY RELEASE AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO) AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO)",568.70000000000005,"TEM",1,"LP",2.5,1]
["3VL37251DC368CD1","CIRCUITBREAKER  VL 250N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=250A, RATED CURRENT IR=200250A, OVERLOAD II=12002500A, SHORTCIRCUIT SHUNT RELEASE 24 V AC/DC AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO)",535.37,"TEM",1,"LP",2.7280000000000002,1]
["3VL37251SP360AD1","CIRCUITBREAKER  VL 250N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, MOTOR/ GENERATOR PROTECTION ELECTRONIC TRIP UNIT ETU10M, LI IN=250A, RATED CURRENT IR=100250A, OVERLOAD II=1,25TO11XIN, SHORTCIRCUIT WITHOUT AUXILIARY RELEASE AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO) AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO)",573.54,"TEM",1,"LP",2.5,1]
["3VL47251DK360AD1","CIRCUITBREAKER  VL 400N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, STARTER COMBINATION PROTECTION OVERCURRENT RELEASE MAGNETIC IN=250A, RATED CURRENT II=20004000A, SHORTCIRCUIT WITHOUT AUXILIARY RELEASE AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO) AUXILIARY/ALARM SWITCH KIT 2HS(1NO+1NC)+1AS(1NO)",695.42,"TEM",1,"LP",5.7,1]
["3VL47312DC360AB1","CIRCUITBREAKER VL 400H HIGH BREAKING CAPACITY ICU=70KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=315A, RATED CURRENT IR=250315A, OVERLOAD II=15753150A, SHORT CIRCUIT WITHOUT AUXILIARY RELEASE AUXILIARY SWITCH KIT 2HS(1NO+1NC)",845.79,"TEM",1,"LP",6.1669999999999998,1]
["3VL47401EE460AA0","CIRCUITBREAKER VL 400N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 4 POLE, NONAUTOMATIC OVERCURRENT RELEASE MAGNETIC IN=400A, RATED CURRENT II=4000A, SHORT CIRCUIT WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",693.33,"TEM",1,"LP",7.88,1]
["3VL47403DC360AA0","CIRCUITBREAKER VL 400L VERY HIGH BREAKING CAPACITY ICU=100KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=400A, RATED CURRENT IR=320400A, OVERLOAD II=20004000A, SHORT CIRCUIT WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",1149.5,"TEM",1,"LP",6.1950000000000003,1]
["3VL57631DC360AC1","CIRCUITBREAKER VL 630N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=630A, RATED CURRENT IR=500630A, OVERLOAD II=32506500A, SHORT CIRCUIT WITHOUT AUXILIARY RELEASE AUXILIARY SWITCH KIT 4HS(2NO+2NC)",1107.7,"TEM",1,"LP",9.3650000000000002,1]
["3VL57632EJ460AA0","CIRCUITBREAKER VL 630H HIGH BREAKING CAPACITY ICU=70KA / 415 V AC 4 POLE, LINE PROTECTION OVERCURRENT RELEASE TM, LI IN=630A, RATED CURRENT IR=500630A, OVERLOAD II=32506500A, SHORT CIRCUIT N  NOT PROTECTED WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",1674.53,"TEM",1,"LP",12.186999999999999,1]
["3VL87161SE300AA0","CIRCUITBREAKER VL 1600N STANDARD BREAKING CAPACITY ICU=55KA / 415 V AC 3 POLE, LINE PROTECTION ELECTRONIC TRIP UNIT ETU20, LSI IN=1600A, RATED CURRENT IR=6401600A, OVERLOAD ISD=1,5TO8XIR, II=9XIN SHORTCIRCUIT WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",4302.76,"TEM",1,"LP",33.479999999999997,1]
["3VL92004WC30","ACCESSORY FOR VL160, DRAW OUT ASSEMBLY FRONT CONNECTORS 3 POLES",257.07,"TEM",1,"LP",4.9870000000000001,1]
["3VL93004PJ00","ACCESSORY FOR VL160X, VL160, VL250, ACCESSORY CONDUCTOR FOR PLUG IN SOCKET",39.82,"TEM",1,"LP",0.19600000000000001,1]
["3VL94001SC00","ACCESSORY FOR VL160X, VL160, VL250, VL400, SHUNT RELEASE 24 V DC RIGHT POLE ONLY",64.790000000000006,"TEM",1,"LP",0.1,1]
["3VL94004PJ00","ACCESSORY FOR VL400, ACCESSORY CONDUCTOR FOR PLUG IN SOCKET",47.19,"TEM",1,"LP",0.215,1]
["3VL95638TC00","ACCESSORY FOR VL630, CURRENT TRANSFORMER FOR OVERLOAD PROTECTION OF THE NCONDUCTOR AND FOR EARTHFAULT PROTECTION IN=630A",225.94,"TEM",1,"LP",0.77100000000000002,1]
["3VL98001SC00","ACCESSORY FOR VL630, VL800, VL1250, VL1600, SHUNT RELEASE 24 V DC RIGHT POLE ONLY",122.1,"TEM",1,"LP",0.151,1]
["3VL11101KM300AA0","CIRCUIT BREAKER VL 150X UL, TYPE CG (CAT NO. NCX3B100) NONINTERCHANGEABLE FRAME W/APPROVAL CIRCUIT BREAKER TO UL489 STANDARD BREAKING CAPACITY 3POLE, NEMA RATING 35KA/480V (MOLDED CASE CIRCUIT BREAKER) OVERCURRENT RELEASE TM, LI FUNCTION TU=40DEGR CELSIUS IN=<100A RATED CURRENT II=1000A SHORTCIRCUIT PROT. IR=100A OVERCURRENT RELEASE FOR SYSTEM PROTECTION W/O CONNECTION ACCESSORIES WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",259.58999999999997,"TEM",1,"LP",2,1]
["3VL94002AB01","ACCESSORY FOR VL150XUL, VL150UL VL250UL, VL400UL,VL400XUL (CGFRAME  LGFRAME) AUX. SWITCH ASSEMBLY KIT 2 AC (1NO+1NC) FOR INSTALL. NPOLE/LEFT/RIGHT",40.049999999999997,"TEM",1,"LP",5.3999999999999999E-2,1]
["3WL11062CB461AA2","WITHDRAWABLE CIRCUIT BREAKER WITH GUIDE FRAME 4POLE, SIZE I, IEC IN=630A TO 690V, AC50/60HZ ICU=55KA AT 500V REAR CONNECTION HORIZONTAL ELECTRONIC TRIP UNIT ETU 25 LSI PROT. ADJUST.B.  0.41 IN W. MAN. OPER. MECHAN. & STORAGE WITH MECHANICAL REQUEST WITHOUT 1ST SHUNT TRIP WITHOUT 2ND SHUNT TRIP 2NO+2NC 2NO+2NC",5718.38,"TEM",1,"LP",84,1]
["3WL11102EB311AA2","FIXEDMOUNTED CIRCUIT BREAKER 3POLE, SIZE I, IEC IN=1000A TO 690V, AC50/60HZ ICU=55KA AT 500V REAR CONNECTION VERTICAL ELECTRONIC TRIP UNIT ETU 45 LSIN PROT. ADJUST.B.  0.41 IN WITH CUBICLE BUS COMMUN./MEASURING FUNCT../ W. MAN. OPER. MECHAN. & STORAGE WITH MECHANICAL REQUEST WITHOUT 1ST SHUNT TRIP WITHOUT 2ND SHUNT TRIP 2NO+2NC 2NO+2NC",3703.23,"TEM",1,"LP",43,1]
["3WL11162BB361AA2","WITHDRAWABLE CIRCUIT BREAKER WITH GUIDE FRAME 3POLE, SIZE I, IEC IN=1600A TO 690V, AC50/60HZ ICU=55KA AT 500V REAR CONNECTION HORIZONTAL ELECTRONIC TRIP UNIT ETU 15 LI PROT. ADJUST.B.  0.51 IN W. MAN. OPER. MECHAN. & STORAGE WITH MECHANICAL REQUEST WITHOUT 1ST SHUNT TRIP WITHOUT 2ND SHUNT TRIP 2NO+2NC 2NO+2NC",5663.52,"TEM",1,"LP",70,1]
["3WL12163CB321AA2","FIXEDMOUNTED CIRCUIT BREAKER 3POLE, SIZE II, IEC IN=1600A TO 690V, AC50/60HZ ICU=80KA AT 500V REAR CONNECTION HORIZONTAL ELECTRONIC TRIP UNIT ETU 25 LSI PROT. ADJUST.B.  0.41 IN W. MAN. OPER. MECHAN. & STORAGE WITH MECHANICAL REQUEST WITHOUT 1ST SHUNT TRIP WITHOUT 2ND SHUNT TRIP 2NO+2NC 2NO+2NC",5417.19,"TEM",1,"LP",56,1]
["3WL12252AA331AA2","FIXEDMOUNT NONAUT. CIRCUITB. 3POLE, SIZE II, IEC IN=2500A TO 690V, AC50/60HZ ICU=66KA AT 500V FRNT.CONN. TOP/BOT. SINGLEHOLE WITHOUT OVERCURRENT TRIP W. MAN. OPER. MECHAN. & STORAGE WITH MECHANICAL REQUEST WITHOUT 1ST SHUNT TRIP WITHOUT 2ND SHUNT TRIP 2NO+2NC 2NO+2NC",6412.86,"TEM",1,"LP",59,1]
["3WL12323AA321AA2","FIXEDMOUNT NONAUT. CIRCUITB. 3POLE, SIZE II, IEC IN=3200A TO 690V, AC50/60HZ ICU=80KA AT 500V REAR CONNECTION HORIZONTAL WITHOUT OVERCURRENT TRIP W. MAN. OPER. MECHAN. & STORAGE WITH MECHANICAL REQUEST WITHOUT 1ST SHUNT TRIP WITHOUT 2ND SHUNT TRIP 2NO+2NC 2NO+2NC",7781.13,"TEM",1,"LP",64,1]
["3WL91110AA620AA0","ACCESSORIES CIRCUIT BREAKER 3WL RATED CURRENT REF. MODULE 2000A F. ETU25, 27, 45, 55, 75, 76",214.66,"TEM",1,"LP",0.01,1]
["3WL91110BA710AA0","ACCESSORIES CIRCUIT BREAKER 3WL LOCKING DEVICE F. MANUAL DRIVE LEVER",143.66,"TEM",1,"LP",0.08,1]
["3WL91110BB270AA0","ACCESSORIES CIRCUIT BREAKER 3WL BOWDEN WIRE F. MUTUAL MECH. INTERLOCKINGS, 4.5M, THREAD M5",207.72,"TEM",1,"LP",0.4,1]
["3WL11102FB321AA2","FIXEDMOUNTED CIRCUIT BREAKER 3POLE, SIZE I, IEC IN=1000A TO 690V, AC50/60HZ ICU=55KA AT 500V REAR CONNECTION HORIZONTAL ELECTRONIC TRIP UNIT ETU 45 LSIN PROT ADJUST. 0.41 IN WITH DISPLAY AND CUBICLE BUS COMM./MEASURING FUNC./EARTH FLT./ZSS OPTION W. MAN. OPER. MECHAN. & STORAGE WITH MECHANICAL REQUEST WITHOUT 1ST SHUNT TRIP WITHOUT 2ND SHUNT TRIP 2NO+2NC 2NO+2NC",3620.43,"TEM",1,"LP",43,1]
["3WL11162CB321AA2","FIXEDMOUNTED CIRCUIT BREAKER 3POLE, SIZE I, IEC IN=1600A TO 690V, AC50/60HZ ICU=55KA AT 500V REAR CONNECTION HORIZONTAL ELECTRONIC TRIP UNIT ETU 25 LSI PROT. ADJUST.B.  0.41 IN W. MAN. OPER. MECHAN. & STORAGE WITH MECHANICAL REQUEST WITHOUT 1ST SHUNT TRIP WITHOUT 2ND SHUNT TRIP 2NO+2NC 2NO+2NC",4608.8599999999997,"TEM",1,"LP",43,1]
["3WL12202AA321AA2","FIXEDMOUNT NONAUT. CIRCUITB. 3POLE, SIZE II, IEC IN=2000A TO 690V, AC50/60HZ ICU=66KA AT 500V REAR CONNECTION HORIZONTAL WITHOUT OVERCURRENT TRIP W. MAN. OPER. MECHAN. & STORAGE WITH MECHANICAL REQUEST WITHOUT 1ST SHUNT TRIP WITHOUT 2ND SHUNT TRIP 2NO+2NC 2NO+2NC",6314.43,"TEM",1,"LP",56,1]
["3WL12252BB321AA2","FIXEDMOUNTED CIRCUIT BREAKER 3POLE, SIZE II, IEC IN=2500A TO 690V, AC50/60HZ ICU=66KA AT 500V REAR CONNECTION HORIZONTAL ELECTRONIC TRIP UNIT ETU 15 LI PROT. ADJUST.B.  0.51 IN W. MAN. OPER. MECHAN. & STORAGE WITH MECHANICAL REQUEST WITHOUT 1ST SHUNT TRIP WITHOUT 2ND SHUNT TRIP 2NO+2NC 2NO+2NC",7046.28,"TEM",1,"LP",59,1]
["3WL12323BB321AA2","FIXEDMOUNTED CIRCUIT BREAKER 3POLE, SIZE II, IEC IN=3200A TO 690V, AC50/60HZ ICU=80KA AT 500V REAR CONNECTION HORIZONTAL ELECTRONIC TRIP UNIT ETU 15 LI PROT. ADJUST.B.  0.51 IN W. MAN. OPER. MECHAN. & STORAGE WITH MECHANICAL REQUEST WITHOUT 1ST SHUNT TRIP WITHOUT 2ND SHUNT TRIP 2NO+2NC 2NO+2NC",8686.76,"TEM",1,"LP",64,1]
["3WL91110AB010AA0","ACCESSORIES CIRCUIT BREAKER 3WL KNIFE STRIP",69.66,"TEM",1,"LP",0.1,1]
["3WL91110AL020AA0","ACCESSORIES CIRCUIT BREAKER 3WL MAIN CONDUCTOR CONN. 1 PIECE FIXEDMOUNTED CIRC.BR. SIZE I FRONT CONN. TOP SINGLEHOLE FRONT ACCESSIBLE UP TO1600A",51.75,"TEM",1,"LP",1.6,1]
["3WL91110BB210AA0","ACCESSORIES CIRCUIT BREAKER 3WL MUTUAL MECHANICAL INTERLOCK W. CABLE PULL 2M FOR FIXED MOUNT. SWITCH",523.09,"TEM",1,"LP",2.7,1]
["3VT17062DC360AA0","CIRCUIT BREAKER 3VT1 STANDARD BREAKING CAPACITY ICU=25KA, 415V AC 3POLE, SYSTEM PROTECTION OVERCURRENT RELEASE TM, LI IN= 63A RATED CURRENT IR= 50... 63A  OVERLOAD PROT. II= 315... 630A, SHORTCIRCUIT PROTECTION WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",107.26,"TEM",1,"LP",1.032,1]
["3VT91002AB10","ACCESSORY FOR VT160 AUX. SWITCH 1CO VT160 60  250V AC/DC",12.02,"TEM",1,"LP",0.02,1]
["3VT92004PA30","ACCESSORY FOR VT250 PLUGIN BASE FRONT CONNECTION 3POLE",91.91,"TEM",1,"LP",1.764,1]
["3VT93003HA10","ACCESSORY FOR VT630 FRONTOP.ROT.OP.MECH. W/O PLUG W/SHAFT END W/O SELECTOR SWITCH ADDIT.SHAFT, MASKING FRAME AND SELECTOR SWITCH REQUIRED",70.09,"TEM",1,"LP",0.308,1]
["3VT93636BC00","ELECTRONIC TRIP UNIT VT630 4POLE, SYSTEM PROTECTION ETU DPN, LI IR= 250...630A, OVERLOAD PROTECTION IRM= 2...9KA, SHORTCIRCUIT PROTECTION, NEUTRAL CONDUCTOR PROTECT. IRN=0.5 TO 1X IR SCREW TERMINAL CONNECTIONS IN SCOPE OF SUPPLY OF SWITCHING UNIT",747.3,"TEM",1,"LP",0.307,1]
["3VT17062DC360AA0","CIRCUIT BREAKER 3VT1 STANDARD BREAKING CAPACITY ICU=25KA, 415V AC 3POLE, SYSTEM PROTECTION OVERCURRENT RELEASE TM, LI IN= 63A RATED CURRENT IR= 50... 63A  OVERLOAD PROT. II= 315... 630A, SHORTCIRCUIT PROTECTION WITHOUT AUXILIARY RELEASE WITHOUT AUXILIARY/ALARM SWITCH",107.26,"TEM",1,"LP",1.032,1]
["3VT92004ED30","ACCESSORY FOR VT250 FRONT CONNECTION BARS INCREASED POLE SPACING COMPRISES 3 TERMINALS SHORT 3POLE",29.59,"TEM",1,"LP",0.29899999999999999,1]
["3VT93003HF20","ACCESSORY FOR VT250, VT630 ACTUATOR WITH PLUG RED/YELLOW",12.42,"TEM",1,"LP",0.08,1]
["3VT93636AS00","ELECTRONIC TRIP UNIT VT630 3POLE,MOTOR/TRANSF.PROTECT. ETU MPS, LSI IR= 250... 630A, OVERLOAD PROTECTION IRM= 3... 9KA SHORTCIRCUIT PROTECTION, SCREW TERMINAL CONNECTIONS IN SCOPE OF SUPPLY OF SWITCHING UNIT",703.36,"TEM",1,"LP",0.30399999999999999,1]
["XPT:8PT11049","CHANGER D3 B 6 W9 LD CHERRY",20.9,"TEM",1,"LP",1.2E-2,0]
["XPT:8PT455","BOTTOM PLATE 200/600",41.08,"TEM",1,"LP",1.917,0]
["XPT:8PT8151","LEVER_6",7.5,"TEM",1,"LP",1.2E-2,0]
["8PQ20206BA22","SIVACON S4 COVER SENTRON 3VT SWITCH 3VT2 UP TO 250A 4POLE ARRANGEMENT HORIZONTAL FIXED MOUNTED, PLUG IN SOCKET UNIVERSAL DRIVE NUMBER OF SWITCHES 1 HEIGHT 200MM WIDTH 600MM",109.61,"TEM",1,"LP",1.02,0]
["8PQ23028BA01","SIVACON S4 TOP PLATE DEGREE OF PROTECTION IP55 BLANK WIDTH 1200MM DEPTH 800MM",215.8,"TEM",1,"LP",12,0]
["8PQ30001BA31","SIVACON S4, section division, for main busbar at top, 1600 mm, D: 400 mm, galvanized",21.11,"TEM",1,"LP",0.23400000000000001,0]
["8PQ12068BA01","SIVACON S4, frame, H: 2000 mm, W: 600 mm, D: 800 mm, galvanized",602.37,"TEM",1,"LP",33.4,0]
["8PQ20606BA06","SIVACON S4 MODULE DOOR DEGREE OF PROTECTION IP4X HEIGHT 600MM WIDTH 600MM",223.56,"TEM",1,"LP",6.48,0]
["8PQ24208BA01","SIVACON S4 REAR WALL DEGREE OF PROTECTION IP55 HEIGHT 2000MM WIDTH 800MM",313.61,"TEM",1,"LP",23,0]
["8PQ50002BA63","SIVACON S4 SUPPORT RAIL HEIGHT 25MM FOR FRAME DEPTH 500, 600, 800MM",17.28,"ΣΥΣΚΕΥΑΣΙΑ",1,"LP",0.312,0]
["8PQ91106AA51","TERMINAL BLOCK HCTBD4FRONT2,58",123.79,"TEM",1,"LP",0.14399999999999999,0]
["8PQ91106AA53","TERMINAL BLOCK HCD40ESTCRDOPE",15.94,"TEM",1,"LP",4.2000000000000003E-2,0]
["5SL61636","CIRCUIT BREAKER 230/400V 6KA, 1POLE, B, 63A",9.94,"TEM",1,"LP",0.161,1]
["5SL61087","CIRCUIT BREAKER 230/400V 6KA, 1POLE, C, 8A",6.05,"TEM",1,"LP",0.13300000000000001,1]
["5SL63637","CIRCUIT BREAKER 400V 6KA, 3POLE, C, 63A",43.12,"TEM",1,"LP",0.48099999999999998,1]
["5SL62067","CIRCUIT BREAKER 400V 6KA, 2POLE, C, 6A",15.46,"TEM",1,"LP",0.247,1]
["5SL63087","CIRCUIT BREAKER 400V 6KA, 3POLE, C, 8A",23.18,"TEM",1,"LP",0.376,1]
["5SL66207","CIRCUIT BREAKER 400V 6KA, 3+NPOLE, C, 20A",28.56,"TEM",1,"LP",0.60399999999999998,1]
["5SL41206","CIRCUIT BREAKER 230/400V 10KA, 1POLE, B, 20A",8.2899999999999991,"TEM",1,"LP",0.16200000000000001,1]
["5SL45207","CIRCUIT BREAKER 230V 10KA, 1+NPOLE, C, 20A",15.21,"TEM",1,"LP",0.312,1]
["5SL44637","CIRCUIT BREAKER 400V 10KA, 4POLE, C, 63A",83.11,"TEM",1,"LP",0.65,1]
["5SL41028","CIRCUIT BREAKER 230/400V 10KA, 1POLE, D, 2A",23.18,"TEM",1,"LP",0.159,1]
["7KM42120BA003AA0","SENTRON, measuring instrument, 7KM PAC4200, LCD, LL: 690 V, LN: 400 V, MODBUS TCP, optional Modbus RTU / PROFINET / PROFIBUS / DI/DO, apparent / active / reactive energy / cos phi, harmonics: 3rd  31st, THD, Cl. 0.2 acc. to IEC61557 12 or Cl. 0.2S acc. to IEC6205322",1408.8,"TEM",1,"LP",0.54600000000000004,1]
["3VA22257HL320AA0","CIRCUIT BREAKER 3VA2 IEC FRAME 250 BREAKING CAPACITY CLASS  C ICU=110KA @ 415 V 3POLE, LINE PROTECTION ETU320, LI, IN=250A OVERLOAD PROTECTION IR=100A ...250A SHORT CIRCUIT PROTECTION II=1,5...10 X IN BUSBAR CONNECTION",839.79,"TEM",1,"LP",2.246,1]
["3VA11103ED120AA0","CIRCUIT BREAKER 3VA1 IEC FRAME 160 BREAKING CAPACITY CLASS  N ICU=25KA @ 240 V 1POLE, LINE PROTECTION TM210,  FTFM, IN=100A OVERLOAD PROTECTION IR=100A FIXED SHORT CIRCUIT PROTECTION II=10 X IN BUSBAR CONNECTION",68.209999999999994,"TEM",1,"LP",0.36,1]
["3VA92140RL20","RCD MODULE RCD520 BASIC RCD TYPE A LOAD SIDE MOUNTED ADJUSTABLE 0,03...5A AT 50/60HZ ADJUSTABLE TV 0...1000MSEC 4 POLE IN=250A UE=100480V ACCESSORY FOR: 3VA1",713.22,"TEM",1,"LP",1.55,1]
["3VA99880BL30","SHUNT TRIP LEFT 24 V AC 50/60 HZ / 2430 V DC ACCESSORY FOR 3VA1/2",53.82,"TEM",1,"LP",8.6999999999999994E-2,1]
["3VA99880AB32","SHORT CIRCUIT ALARM SWITCH CHANGEOVER CONTACTS TYPE HQ (7MM) ACCESSORY FOR: 3VA1 160",22.56,"TEM",1,"LP",2.4E-2,1]
["3KD93046","ACCESSORY FOR 3KD FRAME SIZE 3 CABLE CONNECTION COVER STANDARD LENGTH CONTAINS 6 PC",37.619999999999997,"TEM",1,"LP",0.56000000000000005,1]
["3KD93046","ACCESSORY FOR 3KD FRAME SIZE 3 CABLE CONNECTION COVER STANDARD LENGTH CONTAINS 6 PC",37.619999999999997,"TEM",1,"LP",0.56000000000000005,1]
["5SJ62206KS","CIRCUIT BREAKER 400V 6KA, 2POLE, B, 20A, D=70MM WITH SCREWLESS TAPOFF TERMINAL",14.49,"TEM",1,"LP",0.24399999999999999,1]
["5SY63406","CIRCUIT BREAKER 400V 6KA, 3POLE, B,40A, D=70MM",51.24,"TEM",1,"LP",0.47499999999999998,1]
["5SY61327","CIRCUIT BREAKER 230/400V 6KA, 1POLE, C, 32A, D=70MM",9.31,"TEM",1,"LP",0.154,1]
["5SY63207","CIRCUIT BREAKER 400V 6KA, 3POLE, C, 20A, D=70MM",30.83,"TEM",1,"LP",0.46400000000000002,1]
["5SY66327","CIRCUIT BREAKER 400V 6KA,3+NPOLE C, 32A, D=70MM",46.15,"TEM",1,"LP",0.627,1]
["5SY60407","CIRCUITBREAKER 230 V 6 KA, 1+NPOLE/1MW, C 40A",19.649999999999999,"TEM",1,"LP",0.127,1]
["5SY62257","CIRCUIT BREAKER 400V 6KA, 2POLE, C, 25A, D=70MM",21.53,"TEM",1,"LP",0.31,1]
["5SY65507","CIRCUIT BREAKER 230V 6KA,1+NPOLE C, 50A, D=70MM",26.32,"TEM",1,"LP",0.32900000000000001,1]
["5SY42636","CIRCUIT BREAKER 400V 10KA, 2POLE, B, 63A, D=70MM",52.69,"TEM",1,"LP",0.34,1]
["5SP42806","CIRCUIT BREAKER 400V 10KA, 2POLE, B, 80A, D=70MM",103.18,"TEM",1,"LP",0.53300000000000003,1]
["5SY44406","CIRCUIT BREAKER 400V 10KA, 4POLE, B, 40A, D=70MM",73.150000000000006,"TEM",1,"LP",0.627,1]
["5SP44927","CIRCUIT BREAKER 400V 10KA, 4POLE, C, 125A, D=70MM",125.49,"TEM",1,"LP",1.038,1]
["5SY42637","CIRCUIT BREAKER 400V 10KA, 2POLE, C, 63A, D=70MM",44.84,"TEM",1,"LP",0.34100000000000003,1]
["5SY45257","CIRCUIT BREAKER 230V 10KA, 1+NPOLE, C, 25A, D=70MM",15.32,"TEM",1,"LP",0.315,1]
["5SP43927","CIRCUIT BREAKER 400V 10KA, 3POLE, C, 125A, D=70MM",85.63,"TEM",1,"LP",0.78100000000000003,1]
["5SP44917","CIRCUIT BREAKER 400V 10KA, 4POLE, C, 100A, D=70MM",113.46,"TEM",1,"LP",1.0329999999999999,1]
["5SY45037","CIRCUIT BREAKER 230V 10KA, 1+NPOLE, C, 3A, D=70MM",17.010000000000002,"TEM",1,"LP",0.313,1]
["5SY52057","CIRCUIT BREAKER CURR. SENS DC 440V AC 400V 10KA, 2POLE, C, 0.5A",55.84,"TEM",1,"LP",0.32900000000000001,1]
["5ST2510","TERMINAL LINK FOR DISTRIBUTORS 5ST2508",4.9800000000000004,"TEM",1,"LP",5.7000000000000002E-2,10]
["5ST3613","PIN BUSBAR, 10 SQMM CONNECTION: 2X3 PHASE SAFETOTOUCH",3.85,"TEM",1,"LP",3.4000000000000002E-2,10]
["5ST3730","PIN BUSBAR SHOCKPROOF, 10 SQMM 1PHASE, 214 MM LONG CAN BE CUT, WITH END CAPS",4.04,"TEM",1,"LP",3.3000000000000002E-2,1]
["5ST3801","BLOCKING FOR HANDLE FOR LSSWITCH DEPTH=70MM FOR 5SY, 5SP, 5TE8",6.96,"TEM",1,"LP",1.2E-2,1]
["5ST2506","CONNECT. F.DISTRIBUTORS 5ST2505 SHOCKHAZARD, 20SQMM 1PHASE, 32MM",2.91,"TEM",1,"LP",1.4999999999999999E-2,10]
["5ST3621","PIN BUSBAR, 10 SQMM CONNECTION: 2X4PHASE SAFETOTOUCH",6.2,"TEM",1,"LP",5.3999999999999999E-2,10]
["5ST3715","PIN BUS BAR SHOCKHAZARD SAFETY, 16QMM 4 PHASE, L= 214MM CAN BE CUT, WITH END CAPS",18.239999999999998,"TEM",1,"LP",0.152,1]
["5ST3806","HANDLE LOCKING DEVICE FOR MCB 5SL, 5SV, 5TL1",3.48,"TEM",1,"LP",4.0000000000000001E-3,5]
["5SY51407KK11","MINIATURE CIRCUITBREAKER UNIV. CUR. DC 220V AC 230/400V 10KA, 1POLE, C, 40A FOR RAILWAY APPLICATIONS",257.39999999999998,"TEM",1,"LP",0.17199999999999999,1]
["5SY51106KK11","MINIATURE CIRCUITBREAKER UNIV. CUR. DC 220V AC 230/400V 10KA, 1POLE, B, 10A FOR RAILWAY APPLICATIONS",128.96,"TEM",1,"LP",0.16900000000000001,1]
["5SL31507","CIRCUIT BREAKER 230/400V 4.5KA, 1POLE, C, 50A",8.59,"TEM",1,"LP",0.16900000000000001,1]
["5SL33207","CIRCUIT BREAKER 400V 4.5KA, 3POLE, C, 20A",19.28,"TEM",1,"LP",0.371,1]
["5SL31027","CIRCUIT BREAKER 230/400V 4.5KA, 1POLE, C, 2A",5.76,"TEM",1,"LP",0.13300000000000001,1]
["5SL32106","CIRCUIT BREAKER 400V 4.5KA, 2POLE, B, 10A",11.32,"TEM",1,"LP",0.252,1]
["5SL34407","CIRCUIT BREAKER 400V 4.5KA, 4POLE, C, 40A",33.01,"TEM",1,"LP",0.61599999999999999,1]
["5SY30207","CIRCUIT BREAKER 230V 4.5KA, 1+NPOLE/1MW, C 20A",27.04,"TEM",1,"LP",0.11,1]
["5SM33450","RCCB, 4pole, type AC, In: 125 A, 30 mA, Un AC: 400 V",483.7,"TEM",1,"LP",0.54700000000000004,1]
["5SM26222","RC unit, 2pole, type AC, selective, In: 40 A, 300 mA, Un AC: 230 V",109.2,"TEM",1,"LP",0.20799999999999999,1]
["5SM37460","RCCB, 4pole, type AC, In: 63 A, 500 mA, Un AC: 400 V",71,"TEM",1,"LP",0.46300000000000002,1]
["5SM33143","RCCB, 2pole, type F, short time delayed, In: 40 A, 30 mA, Un AC: 230 V",154,"TEM",1,"LP",0.27400000000000002,1]
["5SV33446","RCCB, 4pole, type A, In: 40 A, 30 mA, Un AC: 400 V",92.4,"TEM",1,"LP",0.36099999999999999,1]
["5SM33466BA","RCCB, 4pole, type A, In: 63 A, 30 mA, Un AC: 400 V",175.9,"TEM",1,"LP",0.52,1]
["5SM37466","RCCB, 4pole, type A, In: 63 A, 500 mA, Un AC: 400 V",130.5,"TEM",1,"LP",0.46100000000000002,1]
["5SM33244","RCCB, 2pole, type B, short time delayed, In: 40 A, 30 mA, Un AC: 230 V",527.73,"TEM",1,"LP",0.55000000000000004,1]
["5SU16531KK16","RCBO elm, 4,5 kA, 1P+N, type AC, 300 mA, Cchar, In: 16 A, Un AC: 230 V",71.8,"TEM",1,"LP",0.26800000000000002,1]
["5SU13547KK10","RCBO elm, 10 kA, 1P+N, type A, 30 mA, Cchar, In: 10 A, Un AC: 230 V",159.9,"TEM",1,"LP",0.27400000000000002,1]
["5SY41408","CIRCUIT BREAKER 230/400V 10KA, 1POLE, D, 40A, D=70MM",36.49,"TEM",1,"LP",0.16600000000000001,1]
["5SY43408","CIRCUIT BREAKER 400V 10KA, 3POLE, D, 40A, D=70MM",146.59,"TEM",1,"LP",0.48199999999999998,1]
["5SY43018","CIRCUIT BREAKER 400V 10KA, 3POLE, D, 1A, D=70MM",117.49,"TEM",1,"LP",0.47399999999999998,1]
["5SY46408","CIRCUIT BREAKER 400V 10KA, 3+NPOLE, D, 40A, D=70MM",182.76,"TEM",1,"LP",0.64500000000000002,1]
["5SY71506","CIRCUIT BREAKER 230/400V 15KA, 1POLE, B, 50A, D=70MM",20.09,"TEM",1,"LP",0.17,1]
["5TE4808","PUSHBUTTON, 1NO/1NC 20 A 1 BUTTON BLUE WITHOUT LATCHING FUNCTION",10.69,"TEM",1,"LP",7.3999999999999996E-2,1]
["5TE6801","SCHUKO SOCKET 16A WITH COVER ACC. TO DIN VDE 0620 FOR INSTALL. IN DISTRIB. BOARDS",8.2100000000000009,"TEM",1,"LP",9.0999999999999998E-2,1]
["5TL11400","ISOLATOR 40A SINGLE POLE",5.62,"TEM",1,"LP",0.115,1]
["5TE4805","PUSHBUTTON, 1NO/1NC 20 A 1 BUTTON RED WITHOUT LATCHING FUNCTION",10.69,"TEM",1,"LP",7.3999999999999996E-2,1]
["5TE8111","SWITCH, D=70MM 20A 1NO",4.21,"TEM",1,"LP",5.8000000000000003E-2,1]
["5TL12910","ISOLATOR 100A DOUBLE POLE",20.52,"TEM",1,"LP",0.22500000000000001,1]
["7KT5500","TIME COUNT. 48X48MM DC 1080V",49.31,"TEM",1,"LP",5.8000000000000003E-2,1]
["7KT1200","CURRENT TRANSFORMER AC 3X60/5A, DEPTH=70MM",111.06,"TEM",1,"LP",0.53500000000000003,1]
["7LF45212","WEEKLY TIME SWITCH PROFI DIGITAL 24V 16A 1CHANNEL 2MW",112.71,"TEM",1,"LP",0.17399999999999999,1]
["7LF53010","SYNCHRONOUS TIME SWITCH DAY 1 CHANGEOVER CONT.230V/50HZ SURFACE MOUNTING",63.34,"TEM",1,"LP",0.214,1]
["5SD74441","COMBIN. ARRESTER TYPE 1 + 2 REQ.CATEGORIES B+C, UC 350V PLUGIN PROTECTION BLOCKS 4POLE, 3+1 CIRCUIT FOR TNS AND TT SYSTEMS W. REMOTE DISPLAY",860.4,"TEM",1,"LP",1.5069999999999999,1]
["5SP93407KC47","CIRCUIT BREAKER 400V 50KA ACC. IEC 9472, T92 3POLE, C, 40A",126.68,"TEM",1,"LP",0.70899999999999996,2]
["5SY71107","CIRCUIT BREAKER 230/400V 15KA, 1POLE, C, 10A, D=70MM",11.18,"TEM",1,"LP",0.16400000000000001,1]
["5SY81027","CIRCUIT BREAKER 230/400V 25KA, 1POLE, C, 2A, D=70MM",17.39,"TEM",1,"LP",0.16600000000000001,1]
["5SY72107","CIRCUIT BREAKER 400V 15KA, 2POLE, C, 10A, D=70MM",31.36,"TEM",1,"LP",0.317,1]
["5SY81167","CIRCUIT BREAKER 230/400V 25KA, 1POLE, C, 16A, D=70MM",14.59,"TEM",1,"LP",0.159,1]
["5SY73168","CIRCUIT BREAKER 400V 15KA, 3POLE, D, 16A, D=70MM",97.5,"TEM",1,"LP",0.45100000000000001,1]
["5TT3408","VOLTAGE RELAY, NTYPE AC 230/400V 2CO 0.9/1.3+0.7/1.1",237.95,"TEM",1,"LP",0.13200000000000001,1]
["5TT41323","REMOTE SWITCH 2 NO CONTACTS SERIE CONTACT FOR AC 230,400V 16A ACTIVATION AC 12V",39,"TEM",1,"LP",0.14499999999999999,1]
["5TT58020","INSTA CONTACTOR WITH 2 BREAK CONTACTS CONTACT FOR 230, 400 V AC, 20 A TRIGGERING 230 V AC",27.3,"TEM",1,"LP",0.13800000000000001,1]
["5TT42172","RELAY,NTYPE W 2 CHANGEOV.CONT. CONTACT FOR AC 230, 400V 16A CONTROL DC 24V",50.5,"TEM",1,"LP",0.14899999999999999,1]
["5TT41153","REMOTE SWITCH WITH 1 NO AND 1 NC CONTACT FOR AC 230, 400V 16A CONTROL DC 12V",38.9,"TEM",1,"LP",0.14899999999999999,1]
["5TT58306","INSTA CONTACTOR 0/1 AUTOMATIC WITH 4 MAKE CONTACTS CONTACT FOR 230, 400 V AC, 25 A TRIGGERING 230 V AC",34.799999999999997,"TEM",1,"LP",0.253,1]
["3NA3132","LV HRC fuse link, NH1, In: 125 A, gG, Un AC: 500 V, Un DC: 440 V, Front indicator, non insulated grip lugs",9,"TEM",1,"LP",0.28699999999999998,3]
["3NA3805","LV HRC fuse link, NH000, In: 16 A, gG, Un AC: 500 V, Un DC: 250 V, Front indicator, non insulated grip lugs",4.5999999999999996,"TEM",1,"LP",0.13100000000000001,3]
["3NA68104","LV HRC fuse link, NH000, In: 25 A, gG, Un AC: 400 V, Combination indicator, insulated grip lugs",7.3,"TEM",1,"LP",0.13200000000000001,3]
["3NA7817","LV HRC fuse link, NH000, In: 40 A, gG, Un AC: 500 V, Un DC: 250 V, Combination indicator, noninsulated grip lugs",4.2,"TEM",1,"LP",0.127,3]
["3ND2360","LV HRC fuse link, NH3, In: 400 A, AM, Un AC: 690 V, Un DC: 250 V, Front indicator, non insulated grip lugs",89.9,"TEM",1,"LP",0.65900000000000003,3]
["3NA31326","LV HRC fuse link, NH1, In: 125 A, gG, Un AC: 690 V, Un DC: 440 V, Front indicator, non insulated grip lugs",38.299999999999997,"TEM",1,"LP",0.27200000000000002,3]
["3NA38056","LV HRC fuse link, NH000, In: 16 A, gG, Un AC: 690 V, Un DC: 250 V, Front indicator, non insulated grip lugs",24.8,"TEM",1,"LP",0.13,3]
["3NA7814","LV HRC fuse link, NH000, In: 35 A, gG, Un AC: 500 V, Un DC: 250 V, Combination indicator, noninsulated grip lugs",4.2,"TEM",1,"LP",0.13,3]
["3ND1372","LV HRC fuse link, NH3, In: 630 A, AM, Un AC: 690 V, Un DC: 440 V, Front indicator, non insulated grip lugs",105.1,"TEM",1,"LP",1.036,3]
["5SB271","DIAZED FUSE LINK 500V F.CABLE AND LINE PROTECTION OP.CL.GL,SZ.DII,THREAD E27,20A",0.52,"TEM",1,"LP",0.03,25]
["5SF1215","DIAZEDBASE DIII 63A AC690V DC500V SADDLE/SADDLE TERMINAL",8.65,"TEM",1,"LP",0.14399999999999999,5]
["5SH318","DTYPE ADAPTOR SCREW SIZE DIII/THREAD E33, 50A",0.93,"TEM",1,"LP",2.1999999999999999E-2,25]
["5SH5514","END CAP FOR 3PHASE BUSBAR",0.82,"TEM",1,"LP",1E-3,10]
["5SB421","DIAZED FUSE LINK 500V F.CABLE AND LINE PROTECTION",1.65,"TEM",1,"LP",5.0999999999999997E-2,25]
["5SG1655","NEOZED, fuse base, D02, 1pole, 63 A, Un AC: 400 V, Un DC: 250 V, without cover",4.0199999999999996,"TEM",1,"LP",8.5000000000000006E-2,6]
["5SH3703","DPASS SCREW DRIVER",8.14,"TEM",1,"LP",4.5999999999999999E-2,10]
["5SG76310KK16","MINIZED, Fuse switch disconnector, D01, 3pole, In: 16 A, Un AC: 400 V",34.92,"TEM",1,"LP",0.23100000000000001,4]
["3NW10800HG","SENTRON, cylindrical fuse link, Class CC, 8 A, slow, Un AC: 600 V",27.4,"TEM",1,"LP",0.01,10]
["3NW30200HG","SENTRON, cylindrical fuse link, Class CC, 2 A, slow, current limiting, Un AC: 600 V",30.49,"TEM",1,"LP",8.0000000000000002E-3,10]
["3NW61011","SENTRON, cylindrical fuse link, 14 x 51 mm, 6 A, gG, Un AC: 500 V",2.9,"TEM",1,"LP",1.2E-2,10]
["3NW7063","SENTRON, cylindrical fuse holder, 10 x 38 mm, 3P+N, In: 32 A, Un AC: 690 V",25.3,"TEM",1,"LP",0.20300000000000001,1]
["3NW62051","SENTRON, cylindrical fuse link, 22 x 58 mm, 16 A, gG, Un AC: 500 V",5.0999999999999996,"TEM",1,"LP",5.1999999999999998E-2,10]
["3NW62101","SENTRON, cylindrical fuse link, 22 x 58 mm, 25 A, gG, Un AC: 500 V",5.0999999999999996,"TEM",1,"LP",4.4999999999999998E-2,10]
["3NW82301","SENTRON, cylindrical fuse link, 22 x 58 mm, 100 A, AM, Un AC: 400 V",8.5,"TEM",1,"LP",5.5E-2,10]
["3NC84253C","SITOR fuse link, with slotted blade contacts, NH3, In: 200 A, gR, Un AC: 690 V, Un DC: 440 V, Front indicator",174.59,"TEM",1,"LP",1,3]
["3NE14372","SITOR fuse link, with blade contacts, NH3, In: 710 A, gR, Un AC: 690 V, Un DC: 440 V, Front indicator",324.55,"TEM",1,"LP",1.19,3]
["3NE4102","SITOR fuse link, with blade contacts, NH0, In: 40 A, gR, Un AC: 1000 V, Un DC: 250 V, Front indicator",45.84,"TEM",1,"LP",0.26900000000000002,3]
["3NE56330C","SITOR fuse link, with slotted blade contacts, NH3, In: 450 A, aR, Un AC: 1500 V, Un DC: 900 V, Front indicator",393.25,"TEM",1,"LP",1.595,3]
["3NC1425","SITOR cylindrical fuse link, 14 x 51 mm, 25 A, aR, Un AC: 690 V, Un DC: 800 V, DC acc. to UL",13.49,"TEM",1,"LP",2.1000000000000001E-2,10]
["3NE12250","SITOR fuse link, with blade contacts, NH1, In: 200 A, gS, Un AC: 690 V, Un DC: 250 V, Front indicator",157.08000000000001,"TEM",1,"LP",0.58299999999999996,3]
["3NE3231","SITOR fuse link, with slotted blade contacts, NH1, In: 350 A, aR, Un AC: 1000 V, Front indicator",130.91,"TEM",1,"LP",0.59599999999999997,3]
["3NE54260C","SITOR fuse link, with slotted blade contacts, NH3, In: 224 A, aR, Un AC: 1500 V, Un DC: 1000 V, Front indicator",341.65,"TEM",1,"LP",1.986,2]
["5SH2242","PROTECTIVE COVER ISO FOR REITER FUSE BASE 3POLE FOR 60 MM BUSBAR SYSTEM DIII/63A 1FOLD",2.37,"TEM",1,"LP",5.8999999999999997E-2,2]
["5SM16140","RCCB, 2pole, type AC, In: 40 A, 300 mA, Un AC: 230 V",53.05,"TEM",1,"LP",0.23100000000000001,1]
["8GF5761","STAB UNIVERSAL BUSBAR SUPPORT 4POLE STAGED, 30X10MM",87.76,"TEM",1,"LP",0.39700000000000002,1]
["8WH10000AN00","HIGHCURRENT TERMINAL WITH SCREW CONNECTION, SECTION: 25  50 MM2, , AWG: 6  1/0, WIDTH: 20 MM, COLOR: GRAY",9.7899999999999991,"TEM",1,"LP",0.125,10]
["8WH10600AQ00","TAB TERMINAL WITH BOLT CONNECTION, SECTION: 0  95 MM2, AWG: 2  4/0, WIDTH: 40 MM, COLOR: GRAY",13.8,"TEM",1,"LP",0.30299999999999999,10]
["8WH20006AG00","ISOLATING TERMINAL WITH SPRING CONNECTION, SECTION: 0.5  4  MM2, WIDTH: 6.2 MM, COLOR: GRAY",2,"TEM",1,"LP",0.01,50]
["8WH20040AE00","FEEDTHROUGH TERMINAL WITH SPRING CONNECTION, 4 CONNECT. POINTS, SECTION: 0.14  1.5 MM2, WIDTH: 4.2 MM, COLOR: GRAY",0.9,"TEM",1,"LP",8.0000000000000002E-3,50]
["8WH25030AH00","FEEDTHROUGH TERMINAL WITH SPRING CONNECTION, COMPACT DESIGN, 3 CONNECT. POINTS SECTION: 0.2  6 MM2, WIDTH: 8.2 MM, COLOR: GRAY",2.1,"TEM",1,"LP",2.1000000000000001E-2,50]
["8WH20000AG06","FEEDTHROUGH TERMINAL WITH SPRING CONNECTION, SECTION: 4 SQMM, WIDTH: 6,2 MM, COLOR:YELLOW",0.8,"TEM",1,"LP",8.9999999999999993E-3,50]
["8WH20030AF00","FEEDTHROUGH TERMINAL WITH SPRING CONNECTION, 3 CONNECT. POINTS SECTION: 0.08  2.5 MM2, WIDTH: 5.2 MM, COLOR: GRAY",0.9,"TEM",1,"LP",8.0000000000000002E-3,50]
["8WH20200CF07","TWOTIER PE TERMINAL WITH SPRING CONNECTION, SECTION: 0.08  2.5 MM2, WIDTH: 5.2 MM, COLOR:GREENYEL.",4.9000000000000004,"TEM",1,"LP",1.4999999999999999E-2,50]
["8WH25000AG01","FEEDTHROUGH TERMINAL WITH SPRING CONNECTION, COMPACT DESIGN, SECTION: 0.08  4 MM2, WIDTH: 6.2 MM, COLOR: BLUE",0.9,"TEM",1,"LP",1.0999999999999999E-2,50]
["8WH30000AE01","FEEDTHROUGH TERMINAL WITH QUICK CONNECTION, SECTION: 0.25  1.5 MM2, WIDTH: 5.2 MM, COLOR: BLUE",0.8,"TEM",1,"LP",8.0000000000000002E-3,50]
["8WH81203AA25","LABELS U,V,W,N,  SIZE ZB6",5.4,"TEM",100,"LP",1E-3,100]
["8WH81207XA05","LABELS, LONGIT. SPECIAL LABELLING  ZB15",13.4,"TEM",100,"LP",1E-3,100]
["8WH81401AB05","LABELS, TRANSV. 1  10 SIZE ZB4",5.4,"TEM",100,"LP",1E-3,100]
["8WH81404AB15","LABELS, TRANSV. 11  20 SIZE ZB8",5.4,"TEM",100,"LP",1E-3,100]
["8WH81413XA05","LABELS, FLAT, TRANSV. SPECIAL LABELLING  ZBF6",13,"TEM",100,"LP",1E-3,100]
["8WH90100EB02","MODULAR TEST PLUG, FOR INDIVIDUAL ASSEMBLING OF TEST PLUG CONNECTOR, FOR SPRING TERMINALS WITH 2.5 MM2, COLOR: RED",4.4000000000000004,"TEM",1,"LP",4.0000000000000001E-3,10]
["8WH90206DC10","PLUGIN JUMPER 8 DIVISIONS, AS TRANSVERSE JUMPER IN TERM. MIDDLE, 2POLE, COLOR: SIEMENS COLOR",0.4,"TEM",1,"LP",4.0000000000000001E-3,10]
["8WH90700DA00","COMPARTMENT PARTITION FOR OPTICAL AND ELECTRICAL ISOL. FROM TERMINAL GROUPS, WITH SECTIONS UP TO 6 MM2, WIDTH: 2 MM, COLOR: GRAY",47.7,"TEM",100,"LP",7.0000000000000001E-3,50]
["8WH81203AB55","LABELS, LONGIT. 51  60 SIZE ZB6",5.4,"TEM",100,"LP",1E-3,100]
["8WH81203AC05","LABELS, LONGIT. 91  100 SIZE ZB6",5.4,"TEM",100,"LP",1E-3,100]
["8WH81211AC05","LABELS, FLAT, LONGIT. 91  100 SIZE ZBF4",5.0999999999999996,"TEM",100,"LP",1E-3,100]
["8WH81402AB25","LABELS, TRANSV. 21  30 SIZE ZB5",5.4,"TEM",100,"LP",1E-3,100]
["8WH81411AB75","LABELS, FLAT, TRANSV. 71  80 SIZE ZBF4",5.0999999999999996,"TEM",100,"LP",1E-3,100]
["8WH90002GA00","COVER FOR FEEDTHROUGH TERM. WITH SPRING CONNECTION, 3 CONNECT. POINTS, SECTION: 2.5 MM2, WIDTH: 2.2 MM, COLOR: GRAY",38.1,"TEM",100,"LP",3.0000000000000001E-3,50]
["8WH90200EC10","REDUCING JUMPER, TO CONNECT SPRING CONNECTIONS 35 MM2 WITH SPRING TERMINALS 2.5 MM2 OR 4 MM2, SIEMENS COLOR",1.8,"TEM",1,"LP",8.0000000000000002E-3,10]
["8WH90400BB00","COMPONENT PLUG, CAN BE USED IN ALL SPRING BASIC ISOL. TERMINALS QUICK CONNECTION 1.5  2.5 MM2 AND COMPACT DESIGN 2.5  4 MM2, COLOR: GRAY",2.5,"TEM",1,"LP",4.0000000000000001E-3,10]
["8WH92000AA00","SCREWDRIVER SIZE: 0.4 X 2.5 MM",8.4,"TEM",1,"LP",3.7999999999999999E-2,10]
["8GK10311KK11","ALPHA 160, wallmounted cabinet, flushmounting, IP31, safety class 2, H: 500 mm, W: 300 mm, D: 140 mm, RAL 9016",207.83,"TEM",1,"LP",7.2,1]
["8GK20431KM21","ALPHA 125 UNIVERSAL, wall mounted cabinet, flush mounting, with distribution board panel, IP31, safety class 1, H: 600 mm, W: 600 mm, D: 140 mm, RAL 7035, with door incl. inspection window",701.32,"TEM",1,"LP",20.8,1]
["8WA10111PG11","THROUGHTYPE TERMINAL THERMOPL. SCREW TERMINAL ON BOTH ENDS SINGLE TERM., GREENYELLOW, 6.5MM,4",1.1200000000000001,"TEM",1,"LP",0.01,50]
["8WA10111DG11","THROUGHTYPE TERMINAL THERMOPL. SCREW TERMINAL ON BOTH ENDS SINGLE TERM., 6.5MM SZ 4",0.71,"TEM",1,"LP",0.01,100]
["8WA10111SF12","FUSE TERMINAL THERMOPLASTIC SCREW TERMINAL ON BOTH ENDS 10MM SZ1.5",3.16,"TEM",1,"LP",2.1000000000000001E-2,10]
["8WA1206","THROUGHTYPE TERMINAL THERMOPL. SCREW TERMINAL ON BOTH ENDS SINGLE TERM. 25MM, SZ 70",13.67,"TEM",1,"LP",0.17100000000000001,10]
["8WA18227EF85","G FUSE LINK DIN 41662 TIMELAG LOW BREAKING CAPACITY RATED UNINT. CURRENT 6.3A",1.4,"TEM",1,"LP",1E-3,10]
["8WA83480XA","PLATES HORIZONTEL.TEXT PACK WITH 136 PLATES 2 CARDS PER 68 PLATES INSCRIPTION 2MM SIZE. 5X7MM,",15.3,"TEM",100,"LP",1E-3,136]
["8WA1852","CONNECTING BAR FOR 4 TERMINALS SIZE 4",1.3,"TEM",1,"LP",5.0000000000000001E-3,20]
["8WA1854","TEST SOCKET 2.3MM",0.2,"TEM",1,"LP",1E-3,100]
["5TG18002","DELTA PROFIL COVER PLATE 65X65MM FOR TAE OUTLET BOX AND LOUDSPEAKER OUTLET BOX TITANIUM WHITE",7.65,"TEM",1,"LP",1.4999999999999999E-2,1]
["5TG2561","ISYSTEM, TITANIUM WHITE ANTENNA COVER PLATE 55X55MM F.BROADBAND OUTLET BOX RF/TV",2.65,"TEM",1,"LP",1.3000000000000001E-2,1]
["5TG55310BE","IRIS ROCKER WITH TRANSPERENT WINDOW WITH SYMBOL LIGHT BEIGE",4.3899999999999997,"TEM",1,"LP",2.1000000000000001E-2,1]
["5TG55335BE","IRIS COVER PLATE 40MM FOR LOUDSPEAKERSOCKET, PILOT LIGHT AND PRESENCEDETECTOR BEIGE",4.28,"TEM",1,"LP",0.01,1]
["5TG6277","ISYSTEM, ELECTRIC WHITE ROCKER W. BELL SYMBOL FOR PUSHB., 55X55MM",3.16,"TEM",1,"LP",2.2000000000000002E-2,1]
["5TG7817","DELTA PROFIL, TITANIUM WHITE ROCKER W. WINDOW, W. LAB. PLATE F.2CIRCUIT/DUAL 2WAY SWITCH F. PUSHB. 2FOLD CENTER POSITION FOR DOUBLE PUSHB., 65X65MM",21.01,"TEM",1,"LP",2.7E-2,1]
["5UB4713","DELTA FLAT IP44, SM DARK GRAY/LIGHT GRAY SCHUKO OUTLET 10/16A 250V W. SCREWLESS TERMINALS M.HINGED LID, W. LABEL. FIELD 66X75MM",10.3,"TEM",1,"LP",0.11700000000000001,1]
["5TG11150","DELTA MIRO FRAME 5FOLD COLOUR TITANIUM WHITE DIMENSIONS 374X90MM",29.58,"TEM",1,"LP",7.5999999999999998E-2,1]
["5TG1818","DELTA PROFIL, TITANIUM WHITE COVER PLATE UAECONNECTION BOX SUITABLE F.RUTENBECK CAT.3+5/ BTR CAT.6, 65X65MM",6.43,"TEM",1,"LP",1.7000000000000001E-2,1]
["5TG25932","ISYSTEM COVER PLATE 55X55MM FOR TAE OUTLET BOX A. LOUDSPEAKER OUTLET BOX ELECTRIC WHITE",3.77,"TEM",1,"LP",1.0999999999999999E-2,1]
["5TG55322WH","IRIS COVER PLATE FOR SOCKET OUTLETS POLAR WHITE",1.84,"TEM",1,"LP",2.5999999999999999E-2,1]
["5TG55342WH","IRIS FRAME TRIPLE, HORIZONTAL POLAR WHITE",7.96,"TEM",1,"LP",7.5999999999999998E-2,1]
["5TG6282","ISYSTEM, ELECTRIC WHITE ROCKER W. LAB. PLATE F.2CIRCUIT/DUAL 2WAY SWITCH 55X55MM",6.22,"TEM",1,"LP",1.7999999999999999E-2,1]
["5UB1558","ISYSTEM, ELECTRIC WHITE SCHUKO SOCKET OUTL. 10/16A 250V W. SCREWLESS TERMINALS W. INCREASED TOUCH PROTECTION COVER PLATE 55X55MM",10.61,"TEM",1,"LP",8.4000000000000005E-2,1]
["5TC8903","ISYSTEM, CARBON METALLIC COVER PLATE F. DIMMER W. ROTARY BUTTON 55X55MM",19.38,"TEM",1,"LP",1.9E-2,1]
["5TG55300NS","IRIS ROCKER NEPTUNE STEEL",2.96,"TEM",1,"LP",2.8000000000000001E-2,1]
["5TG55313MA","IRIS ROCKER WITH SYMBOL BELL MERCURY ALUMINIUM",6.22,"TEM",1,"LP",0.04,1]
["5TG55327DG","IRIS COVER PLATE FOR R, TV, SAT SOCKET OUTLETS 2 HOLES ODYSSEY GOLD",5.61,"TEM",1,"LP",2.3E-2,1]
["5TG55338DG","IRIS COVER PLATE FOR TELEPHONE SOCKET 1FOLD WITH SCREWS ODYSSEY GOLD",5.2,"TEM",1,"LP",3.5999999999999997E-2,1]
["5TG55400FA","MEGA ROCKER FUSION ALUMINIUM",3.06,"TEM",1,"LP",2.5000000000000001E-2,10]
["5TG55408SB","MEGA ROCKER WITH TRANSPARENT WINDOW AND SYMBOL LIGHT SAMOA BROWN",6.32,"TEM",1,"LP",0.09,1]
["5TG55423MB","MEGA COVER PLATE FOR SOCKET OUTLETS WITH CHILD PROTECTION MISTY BRONZE",4.3899999999999997,"TEM",1,"LP",5.6000000000000001E-2,1]
["5TG55430PA","MEGA COVER PLATE FOR ADAPTER 1FOLD RJ45, RJ11 PRUSIA ALUMINIUM",9.18,"TEM",1,"LP",0.09,1]
["5TG55440MG","MEGA FRAME TRIPLE, HORIZONTAL MALT GOLD",48.96,"TEM",1,"LP",0.13600000000000001,1]
["5TG6227","ISYSTEM, CARBON METALLIC ROCKER W. BELL SYMBOL FOR PUSHB., 55X55MM",4.3899999999999997,"TEM",1,"LP",1.7000000000000001E-2,1]
["5TG7927","DELTA PROFIL, SILVER ROCKER W. BELL SYMBOL FOR PUSHB., 65X65MM",11.02,"TEM",1,"LP",2.6000000000000002E-2,1]
["5UB55101SB","SOL SCHUKO SOCKET OUTLET GERMAN STANDARD 10A 250V AC WITH CLAWS SILVER, BLACK",8.06,"TEM",1,"LP",0.10299999999999999,10]
["5TG1253","ISYSTEM, ALUMIN.METALLIC ANTENNA COVER PLATE 55X55 F.BROADBAND OUTLET BOX RF/TV",8.98,"TEM",1,"LP",1.3000000000000001E-2,1]
["5TG25536","DELTA ISYSTEM, CARBON METALLIC FRAME, 3FOLD, 222X80MM",15.4,"TEM",1,"LP",3.2000000000000001E-2,1]
["5TG55308NS","IRIS ROCKER WITH TRANSPERENT WINDOW WITH SYMBOL BELL NEPTUNE STEEL",6.32,"TEM",1,"LP",4.2999999999999997E-2,1]
["5TG55335RR","IRIS COVER PLATE 40MM FOR LOUDSPEAKERSOCKET, PILOT LIGHT AND PRESENCEDETECTOR RUBY RED",6.83,"TEM",1,"LP",0.09,1]
["5TG55347NS","IRIS FRAME QUADRUPLE, VERTICAL NEPTUNE STEEL",19.48,"TEM",1,"LP",0.105,1]
["5TG55407FA","MEGA ROCKER WITH TRANSPARENT WINDOW AND SYMBOL BELL FUSION ALUMINIUM",6.32,"TEM",1,"LP",0.09,1]
["5TG55422SB","MEGA COVER PLATE FOR SOCKET OUTLETS SAMOA BROWN",2.96,"TEM",1,"LP",3.1E-2,10]
["5TG55428MB","MEGA COVER PLATE FOR ADAPTER 2FOLD RJ11, 45 WITH LABEL FIELD MISTY BRONZE",10,"TEM",1,"LP",0.09,1]
["5TG55437MG","MEGA FRAME SINGLE, HORIZONTAL MALT GOLD",20.3,"TEM",1,"LP",6.4000000000000001E-2,10]
["5TG6225","ISYSTEM, CARBON METALLIC ROCKER F.2CIRCUIT/DUAL 2WAY SWITCH F. DOUBLE PUSHB., 55X55MM",3.16,"TEM",1,"LP",2.3E-2,1]
["5TG7925","DELTA PROFIL, SILVER ROCKER, 65X65MM F.2CIRCUIT/DUAL 2WAY SWITCH F. DOUBLE PUSHB. F.PUSHB. 2FOLD CENTER POSITION",13.46,"TEM",1,"LP",2.9000000000000001E-2,1]
["5UB1927","ISYSTEM, CARBON METALLIC SCHUKO SOCKET OUTL. 10/16A 250V W. SCREWLESS TERMINALS W. HINGED LID 55X55MM",18.77,"TEM",1,"LP",9.9000000000000005E-2,1]
["5TG11220","DELTA MIRO ALUMINUM FRAME 2FOLD REAL ALUMINUM UNPAINTED DIMENSIONS 161X90MM",75.48,"TEM",1,"LP",0.14000000000000001,1]
["5TG1602","DELTA NATUR, LIGHT OAK FRAME, 2FOLD, 152X81MM",30.5,"TEM",1,"LP",4.3000000000000003E-2,1]
["5TG1684","DELTA NATUR, BEECH FRAME, 4FOLD, 294X81MM",72.62,"TEM",1,"LP",0.08,1]
["5UB1641","DELTA NATUR, DARK OAK SCHUKO SOCKET OUTL. 10/16A 250V W. SCREWLESS TERMINALS W. INCREASED TOUCH PROTECTION COVER PLATE 62X62MM",33.97,"TEM",1,"LP",9.0999999999999998E-2,1]
["5TG11240","DELTA MIRO ALUMINUM FRAME 4FOLD REAL ALUMINUM UNPAINTED DIMENSIONS 303X90MM",171.26,"TEM",1,"LP",0.246,1]
["5TG1610","DELTA NATUR, DARK OAK BLANKING PLATE, 62X62MM",21.93,"TEM",1,"LP",5.8000000000000003E-2,1]
["5TG1677","DELTA NATUR, CHERRY COVER PLATE 62X62MM FOR TELECOMMUNICATION CONNECTION UNITS (TAE)",25.81,"TEM",1,"LP",2.5999999999999999E-2,1]
["5TA55104BE","SOL INTERMEDIATE SWITCH 10A 250V AC WITH CLAWS BEIGE",7.87,"TEM",1,"LP",5.7000000000000002E-2,10]
["5TG4324","ISYSTEM SET OF SEALS IP44 F.SWITCH AND PUSHB. ROCKERS F.2CIRCUIT SWITCH A.DOUBLE PUSHB. (1 SET = 4 INDIV. SEALS)",5.8,"ΣΕΤ",1,"LP",1.6E-2,1]
["5TA55010KK","IRIS,MEGA TWO WAY SP SWITCH WITH METALLIC GRID 10A 250V AC CLAWS",6.83,"TEM",1,"LP",5.6000000000000001E-2,1]
["5TD55102SB","SOL PUSHBUTTON WITH SYMBOL BELL, WINDOW 10A 250V AC WITH CLAWS SILVER, BLACK",17.079999999999998,"TEM",1,"LP",9.2999999999999999E-2,10]
["5UB4650","SCHUKO S. OUTLET W. CAST COVER",52.79,"TEM",1,"LP",0.26300000000000001,1]
["5TD2865","ISYSTEM, CARBON METALLIC LIGHT SIGNAL 250V W. GLOW LAMP COVER PLATE 55X55MM W. RED WINDOW",42.85,"TEM",1,"LP",7.8E-2,1]
["8GB4683","BLANK COVER 12 MW WHITE FLAME RESTISTANT FOR SIMBOX",2.2400000000000002,"TEM",1,"LP",2.8000000000000001E-2,10]
["8GK11024KK22","ALPHA 400, wallmounted cabinet, flat pack, IP43, safety class 1, H: 950 mm, W: 550 mm, D: 210 mm, RAL 9016",250,"TEM",1,"LP",16.8,1]
["8GK11025KK12","ALPHA 400, wallmounted cabinet, flat pack, IP43, safety class 1, H: 1100 mm, W: 300 mm, D: 210 mm, RAL 9016",223.18,"TEM",1,"LP",14,1]
["8GK13028KK42","ALPHA 630, floormounted cabinet, flat pack, IP43, safety class 1, H: 1900 mm, W: 1050 mm, D: 210 mm, RAL 7035",988.9,"TEM",1,"LP",62,1]
["8GK13830KK34","ALPHA 630, marshalling box, IP55, safety class 1, H: 350 mm, W: 800 mm, D: 320 mm, RAL 7035",626.45000000000005,"TEM",1,"LP",14.46,1]
["8GK43514KK22","ALPHA 400/630 DIN, KIT F. INSTALL. MOUNTING DEVICE WITH ROW DISTANCE 150 MM H=600 W=500",160.16999999999999,"TEM",1,"LP",3.17,1]
["8GK45013KK22","ALPHA 400/630 DIN, KIT SPACE COVER WITH SUPPORT H=450 W=500",56.75,"TEM",1,"LP",0.92100000000000004,1]
["8GK44514KK32","ALPHA 400/630 DIN MOUNTING KIT MOUNTING PLATE WITH FIELD COVER WITHOUT CUT H=600 W=750",211.97,"TEM",1,"LP",9,1]
["8GK44011KK21","ALPHA 160 DIN, ASSEMBLY KIT F. TERMINAL BLOCKS W. TERMINAL STRIP, HORIZONTAL, H=150 W=500MM",55.72,"TEM",1,"LP",0.76900000000000002,1]
["8GK95600KK13","ALPHA, rotary handle insert, for wallmounted distribution board",59.95,"TEM",1,"LP",0.28499999999999998,1]
["8GK95610KK02","ALPHA, lock insert, for profile semicylinder",15.55,"TEM",1,"LP",3.5000000000000003E-2,1]
["8GK96500KK00","ALPHA 400/630, BB HOLDER 5POLE; 40MM SYSTEM MOUNTED DIRECT ON STAY",29.56,"TEM",1,"LP",0.22900000000000001,1]
["8GK91208KK00","ALPHA 630 UNIVERSAL, SIDE PANEL, IP43, CLOSED, RAL 7035, H=1600, D=250, 1 SET",568.70000000000005,"ΣΕΤ",1,"LP",10.5,1]
["8GK91258KK13","ALPHA 630 UNIVERSAL, INTERMEDIATE UPRIGHT FOR ENCLOSURE H=2000MM, B=900MM",129.30000000000001,"TEM",1,"LP",5,1]
["8GS40344","ALPHA 400ZS N/N TERMINAL 16POLE, 2 X 25SQMM SCREW TER. 14 X 6SQMM PLUGIN TERMINAL, HORIZONTAL INSTALL. OR VERTICALLY ON BUSBAR, COLOR BLUE",56.3,"TEM",1,"LP",5.5E-2,1]
["5TA55018RR","DELTA IRIS CARD OPERATED 1,2 WAY SWITCH 1 MICROSWITCHES COMPLETE WITH COVER PLATE RUBY RED",27.22,"TEM",1,"LP",7.6999999999999999E-2,1]
["5TG55007KK","CORAL, IRIS, MEGA 6 CONTACTS PHONE SOCKET RJ11 FOR BASIC TELEPHON NETWORKS WITH SPARE METALLIC GRID FIXING BY SCREWS",6.52,"TEM",1,"LP",6.3E-2,10]
["5TG98741CM","DELTA MSYSTEM MODULARJACK SOCKET OUTLET CAT3 RJ11 6/4 W. SHUTTER CARBON METALLIC",12.73,"TEM",1,"LP",2.4E-2,1]
["5TG55006KK","CORAL, IRIS CARD TEMPORIZED ONE WAY SP SWITCH, TWO WAY SP SWITCH WITH SPARE METALLIC GRID 125 230V, 50 60HZ, 10A 6A",29.6,"TEM",1,"LP",7.6999999999999999E-2,1]
["5TG59004KK","CORAL, IRIS, MEGA R,TV, SAT SOCKET, 2 OUTLETS SINGLE WITH SPARE METALLIC GRID WITH CLAWS",11.18,"TEM",1,"LP",0.10299999999999999,1]
["7KT1546","EMETER WITH LCDISPLAY, 3 PHASE,125A,2XS0,2 TARIFFS, DIRECT CONNECTION ZERO SETTING COMMUNICATION CAPABLE",565.52,"TEM",1,"LP",0.70499999999999996,1]
["8MR21701BB","THERMOSTAT RANGE 060 GRAD C 6A/250V AC WITH MAKE CONTACT ELEMENT",25.56,"TEM",1,"LP",5.3999999999999999E-2,1]
["3NP52600EA86","SENTRON, fuse switch disconnector 3NP5, 3pole, NH1, 250 A, for assembly and installation on mounting plate, with highspeed closing feature, screw connection, Fuse monitoring: by 3RV, auxiliary switch at the switch disconnector: 1NO+1NC, auxiliary switch at the fuse monitoring device: 1NO+1NC",789.39,"TEM",1,"LP",5.9619999999999997,1]
["3NY1208","ACCESSORIES FOR FUSE SWITCH DISCONNECTORS 3NP5060 INSTALLATION KIT FOR MOUNTING WITH MOULDEDPLASTIC MASKING FRAME 250 X 149MM",60.75,"TEM",1,"LP",0.51400000000000001,1]
["3NJ49180DA02","ACCESSORIES FOR FUSE LOAD ISOL. SWITCHES 3NJ41 ADAPTER FOR COMB. 3NJ4103 WITH 3NJ4124 ON BUSBAR SPACING 185 MM",60.7,"TEM",1,"LP",0.75900000000000001,1]
["3KX35363BA","ACCESSORIES FOR FUSE SWITCH DISCONNECTORS 3KL53 ASSEMBLY WITH REAR MANUAL OPERATING MECHANISM LOCKABLE RED/YELLOW INCLUDING COVER",162.69999999999999,"TEM",1,"LP",0.87,1]
["3KX35523DB01","TERMINAL COVER FOR 4 POLE SWITCH 3KA504, 3KA514, 3KA524, 3KL504, 3KL524 FOR THREAD M6 CONSISTS OF 8 PIECES",40.880000000000003,"TEM",1,"LP",0.1,1]
["8UC9375","OPERATING MECHANISM FOR FIXED MOUNTING ONTO 3KE44, 3KE45 DISCONNECTORS ACTUATING SHAFT 12X12MM SZ.4,HANDLE RED,(EMERG.STOP)",39.54,"TEM",1,"LP",0.16,1]
["3KE43300GA","SWITCH DISCONNECTOR 3POLE WITH DOOR DRIVE 8UC7 HANDLE TIGREY/BL.GREEN BASIC MASKING FRAME LIGHT GRAY",811.96,"TEM",1,"LP",5.0460000000000003,1]
["3KX31761E","ACCESSORIES FOR FUSE SWITCH DISCONNECTORS 3KA5558, 3KL5557,3KM5557 HANDLE 140MM LONG, BLACK WITH SHAFT 10 X 10MM, 205MM LONG",49.99,"TEM",1,"LP",0.28699999999999998,1]
["8UC6082","SPARE PART FOR ROTARY OPERATING MECHANISM 8UC6 EXTENSION SHAFT 600MM LONG 8 X 8MM",15.63,"TEM",1,"LP",0.26500000000000001,1]
["8UC72106BD","SPARE PART FOR 8UC72126BD26 FOR DOORCOUPLING ROTARY DRIVE FOR CIRCUITBREAKER 3VL 8UC7 DESIGN HANDLE TIGREY, MASKING FRAME LIGHT GRAY",89.94,"TEM",1,"LP",0.2,1]
["3KA71553AA00","SWITCH DISCONNECTOR 3X2000A",1706.09,"TEM",1,"LP",18,1]
["3KX71311AB00","CACHE BORNE EN DESSOUS GR1",10.039999999999999,"TEM",1,"LP",3.4000000000000002E-2,1]
["3KA71223AA00","SWITCH DISCONNECTOR 3X200A",188.78,"TEM",1,"LP",1.4,1]
["3KX71125BA00","C:S PORTE ZW 260MM GR5 1250A",42.33,"TEM",1,"LP",0.53400000000000003,1]
["3NJ69004HJ21","ACCESSORY FOR SWITCH DISCONNECTOR W/FUSE, INLINE, PLUGIN, AMPEREMETER, MOVING IRON 400/5A, CL.1, 0.6 VA DOUBLE OVERLOAD",72.900000000000006,"TEM",1,"LP",9.2999999999999999E-2,1]
["3NP19231BE20","Threetier terminal 3x 2.5  16mm2, for size NH000, NH00 with box terminal, accessories for 3NP1 fuse switch disconnectors",25.15,"TEM",1,"LP",0.13100000000000001,1]
["3NP11631DA11","SENTRON, fuse switch disconnector 3NP1, 3pole, NH3, 630 A, for assembly and installation on mounting plate, Flachanschluss, Fuse monitoring: electromechanical, cover level 70mm",507.15,"TEM",1,"LP",5.3259999999999996,1]
["3LD20641GP53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:16 A, Operational power / at AC23 A at 400 V: 7,5 kW, molded plastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, red/yellow",41.5,"TEM",1,"LP",0.47799999999999998,1]
["3LD21657UB01","SENTRON, 3LD switch disconnector, Selector switch, 3pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, moldedplastic enclosure for metric threaded joint, knoboperated mechanism, black",74.209999999999994,"TEM",1,"LP",0.89400000000000002,1]
["3LD23180TK11","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:160 A, Operational power / at AC23 A at 400 V: 75 kW, floor mounting with door coupling, knoboperated mechanism, black, 4hole mounting of the handle",263.2,"TEM",1,"LP",2.75,1]
["3LD23180TK13","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:160 A, Operational power / at AC23 A at 400 V: 75 kW, floor mounting with door coupling, knoboperated mechanism, red/yellow, 4hole mounting of the handle",263.2,"TEM",1,"LP",2.746,1]
["3LD23183VK13","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 6pole, Iu:160 A, Operational power / at AC23 A at 400 V: 75 kW, floor mounting with door coupling, knoboperated mechanism, red/yellow, 4hole mounting of the handle",561.38,"TEM",1,"LP",4.6639999999999997,1]
["3LD23300TK13","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:160 A, Operational power / at AC23 A at 400 V: 132 kW, Distribution board mounting, knoboperated mechanism, red/yellow, handle directly on switch",234.74,"TEM",1,"LP",2.048,1]
["3LD24050TK11","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:160 A, Operational power / at AC23 A at 400 V: 132 kW, frontmounted, knob operated mechanism, black, 4 hole mounting of the handle",289.18,"TEM",1,"LP",2.097,1]
["3LD24051TL13","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 4pole, Iu:160 A, Operational power / at AC23 A at 400 V: 132 kW, front mounted, knoboperated mechanism, red/yellow, 4hole mounting of the handle",347.66,"TEM",1,"LP",2.605,1]
["3LD24180TK11","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:250 A, Operational power / at AC23 A at 400 V: 132 kW, floor mounting with door coupling, knoboperated mechanism, black, 4hole mounting of the handle",318.47000000000003,"TEM",1,"LP",2.7610000000000001,1]
["3LD24183VK13","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 6pole, Iu:250 A, Operational power / at AC23 A at 400 V: 132 kW, floor mounting with door coupling, knoboperated mechanism, red/yellow, 4hole mounting of the handle",671.82,"TEM",1,"LP",4.5570000000000004,1]
["3LD24300TK13","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:250 A, Operational power / at AC23 A at 400 V: 132 kW, Distribution board mounting, knoboperated mechanism, red/yellow, handle directly on switch",286.8,"TEM",1,"LP",2.0470000000000002,1]
["3LD25040TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, frontmounted, rotary operating mechanism, black, 4 hole mounting of the handle",48.13,"TEM",1,"LP",0.41199999999999998,1]
["3LD25040TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, front mounted, rotary operating mechanism, red/yellow, 4hole mounting of the handle",48.13,"TEM",1,"LP",0.41299999999999998,1]
["3LD25041TL51","SENTRON, 3LD switch disconnector, main switch, 4 pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, frontmounted, rotary operating mechanism, black, 4 hole mounting of the handle",63.03,"TEM",1,"LP",0.48499999999999999,1]
["3LD25041TL53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 4pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, front mounted, rotary operating mechanism, red/yellow, 4hole mounting of the handle",63.03,"TEM",1,"LP",0.49,1]
["3LD25041TP53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, front mounted, 1NC, 1NO, rotary operating mechanism, red/yellow, 4hole mounting of the handle",58.68,"TEM",1,"LP",0.438,1]
["3LD25043VK51","SENTRON, 3LD switch disconnector, main switch, 6 pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, frontmounted, rotary operating mechanism, black, 4 hole mounting of the handle",74.62,"TEM",1,"LP",0.74399999999999999,1]
["3LD25140TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, floor mounting with door coupling, rotary operating mechanism, black, 4 hole mounting of the handle",53.51,"TEM",1,"LP",0.63800000000000001,1]
["3LD25140TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, floor mounting with door coupling, rotary operating mechanism, red/yellow, 4hole mounting of the handle",53.51,"TEM",1,"LP",0.64,1]
["3LD25141TL53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 4pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, floor mounting with door coupling, rotary operating mechanism, red/yellow, 4hole mounting of the handle",64.38,"TEM",1,"LP",0.71699999999999997,1]
["3LD25247UK01","SENTRON, 3LD switch disconnector, Selector switch, 3pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, frontmounted, knob operated mechanism, black, 4 hole mounting of the handle",90.15,"TEM",1,"LP",0.74,1]
["3LD25300TK11","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, Distribution board mounting, knoboperated mechanism, black, handle directly on switch",40.57,"TEM",1,"LP",0.30299999999999999,1]
["3LD25300TK13","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, Distribution board mounting, knoboperated mechanism, red/yellow, handle directly on switch",40.57,"TEM",1,"LP",0.29799999999999999,1]
["3LD25440TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, floor mounting with door coupling, rotary operating mechanism, red/yellow, center mounting 22.5 mm of handle",64.069999999999993,"TEM",1,"LP",0.59,1]
["3LD25450TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, floor mounting with door coupling, rotary operating mechanism, black, center mounting 22.5 mm of handle",64.069999999999993,"TEM",1,"LP",0.68899999999999995,1]
["3LD25450TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, floor mounting with door coupling, rotary operating mechanism, red/yellow, center mounting 22.5 mm of handle",64.069999999999993,"TEM",1,"LP",0.68500000000000005,1]
["3LD25550TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, frontmounted, rotary operating mechanism, black, center mounting 22.5 mm of handle",48.13,"TEM",1,"LP",0.41899999999999998,1]
["3LD25550TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, front mounted, rotary operating mechanism, red/yellow, center mounting 22.5 mm of handle",48.13,"TEM",1,"LP",0.41899999999999998,1]
["3LD25650TB51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, moldedplastic enclosure for metric threaded joint, rotary operating mechanism, black",70.790000000000006,"TEM",1,"LP",0.9,1]
["3LD25650TB53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, molded plastic enclosure for metric threaded joint, rotary operating mechanism, red/yellow",70.790000000000006,"TEM",1,"LP",0.90900000000000003,1]
["3LD25651GP51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, moldedplastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, black",80.010000000000005,"TEM",1,"LP",0.90700000000000003,1]
["3LD25651GP53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, molded plastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, red/yellow",80.010000000000005,"TEM",1,"LP",0.90100000000000002,1]
["3LD25651TC51","SENTRON, 3LD switch disconnector, main switch, 4 pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, moldedplastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, black",82.08,"TEM",1,"LP",0.95299999999999996,1]
["3LD25651TC53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 4pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, molded plastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, red/yellow",82.08,"TEM",1,"LP",0.95899999999999996,1]
["3LD25663VB51","SENTRON, 3LD switch disconnector, main switch, 6 pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, moldedplastic enclosure for metric threaded joint, rotary operating mechanism, black",151.11000000000001,"TEM",1,"LP",2.1360000000000001,1]
["3LD25663VB53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 6pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, molded plastic enclosure for metric threaded joint, rotary operating mechanism, red/yellow",151.11000000000001,"TEM",1,"LP",2.1280000000000001,1]
["3LD25664VD53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 6pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, molded plastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, red/yellow",151.11000000000001,"TEM",1,"LP",2.1379999999999999,1]
["3LD25667UB01","SENTRON, 3LD switch disconnector, Selector switch, 3pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, moldedplastic enclosure for metric threaded joint, knoboperated mechanism, black",182.78,"TEM",1,"LP",2.1640000000000001,1]
["3LD27040TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, frontmounted, rotary operating mechanism, black, 4 hole mounting of the handle",73.069999999999993,"TEM",1,"LP",0.497,1]
["3LD27040TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, front mounted, rotary operating mechanism, red/yellow, 4hole mounting of the handle",73.069999999999993,"TEM",1,"LP",0.49399999999999999,1]
["3LD27041TP53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, front mounted, 1NC, 1NO, rotary operating mechanism, red/yellow, 4hole mounting of the handle",83.63,"TEM",1,"LP",0.51700000000000002,1]
["3LD27140TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, floor mounting with door coupling, rotary operating mechanism, black, 4 hole mounting of the handle",87.77,"TEM",1,"LP",0.755,1]
["3LD27140TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, floor mounting with door coupling, rotary operating mechanism, red/yellow, 4hole mounting of the handle",87.77,"TEM",1,"LP",0.755,1]
["3LD27247UK01","SENTRON, 3LD switch disconnector, Selector switch, 3pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, frontmounted, knob operated mechanism, black, 4 hole mounting of the handle",169.02,"TEM",1,"LP",0.95599999999999996,1]
["3LD27300TK11","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, Distribution board mounting, knoboperated mechanism, black, handle directly on switch",69.66,"TEM",1,"LP",0.375,1]
["3LD27300TK13","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, Distribution board mounting, knoboperated mechanism, red/yellow, handle directly on switch",69.66,"TEM",1,"LP",0.375,1]
["3LD27660TB51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, moldedplastic enclosure for metric threaded joint, rotary operating mechanism, black",160.84,"TEM",1,"LP",1.8859999999999999,1]
["3LD27660TB53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, molded plastic enclosure for metric threaded joint, rotary operating mechanism, red/yellow",160.84,"TEM",1,"LP",1.8939999999999999,1]
["3LD27661GP51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, moldedplastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, black",165.7,"TEM",1,"LP",1.8149999999999999,1]
["3LD27661GP53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, molded plastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, red/yellow",165.7,"TEM",1,"LP",1.8560000000000001,1]
["3LD27667UB01","SENTRON, 3LD switch disconnector, Selector switch, 3pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, moldedplastic enclosure for metric threaded joint, knoboperated mechanism, black",300.56,"TEM",1,"LP",2.3090000000000002,1]
["3LD28040TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:125 A, Operational power / at AC23 A at 400 V: 45 kW, frontmounted, rotary operating mechanism, black, 4 hole mounting of the handle",92.63,"TEM",1,"LP",0.501,1]
["3LD28040TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:125 A, Operational power / at AC23 A at 400 V: 45 kW, front mounted, rotary operating mechanism, red/yellow, 4hole mounting of the handle",92.63,"TEM",1,"LP",0.496,1]
["3LD28041TP53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:125 A, Operational power / at AC23 A at 400 V: 45 kW, front mounted, 1NC, 1NO, rotary operating mechanism, red/yellow, 4hole mounting of the handle",103.19,"TEM",1,"LP",0.51500000000000001,1]
["3LD28140TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:125 A, Operational power / at AC23 A at 400 V: 45 kW, floor mounting with door coupling, rotary operating mechanism, black, 4 hole mounting of the handle",109.71,"TEM",1,"LP",0.752,1]
["3LD28140TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:125 A, Operational power / at AC23 A at 400 V: 45 kW, floor mounting with door coupling, rotary operating mechanism, red/yellow, 4hole mounting of the handle",109.71,"TEM",1,"LP",0.754,1]
["3LD28300TK11","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:125 A, Operational power / at AC23 A at 400 V: 45 kW, Distribution board mounting, knoboperated mechanism, black, handle directly on switch",89.32,"TEM",1,"LP",0.374,1]
["3LD28300TK13","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:125 A, Operational power / at AC23 A at 400 V: 45 kW, Distribution board mounting, knoboperated mechanism, red/yellow, handle directly on switch",89.32,"TEM",1,"LP",0.378,1]
["3LD28660TB53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:125 A, Operational power / at AC23 A at 400 V: 45 kW, molded plastic enclosure for metric threaded joint, rotary operating mechanism, red/yellow",291.66000000000003,"TEM",1,"LP",1.883,1]
["3LD28661GP53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:125 A, Operational power / at AC23 A at 400 V: 45 kW, molded plastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, red/yellow",300.56,"TEM",1,"LP",1.819,1]
["3LD92002B","neutral conductor/PE terminal, throughtype, for front mounting, up to 16A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",6.93,"TEM",1,"LP",0.03,1]
["3LD92005B","Auxiliary switch, 1NO+1NC, lagging switching, Accessories for 3LD2 main control and EMERGENCYSTOP switches",10.66,"TEM",1,"LP",0.02,1]
["3LD92005C","Auxiliary switch, 1NO+1NC, Accessories for 3LD2 main control and EMERGENCYSTOP switches",10.66,"TEM",1,"LP",0.02,1]
["3LD92006C","Auxiliary switch, 2NO, Accessories for 3LD2 main control and EMERGENCYSTOP switches",11.9,"TEM",1,"LP",2.1000000000000001E-2,1]
["3LD92050C","shaft set, for rotary operating mechanism with door coupling, shaft 6x6mm, length 300 mm, Accessories for 3LD2 main control and EMERGENCY STOP switches",6.42,"TEM",1,"LP",0.47899999999999998,5]
["3LD92052C","shaft set, for rotary operating mechanism shaft 6x6mm, length 600mm, Accessories for 3LD2 main control and EMERGENCYSTOP switches",12.52,"TEM",1,"LP",0.84299999999999997,5]
["3LD92200B","neutral conductor, leading switching for front mounting, up to 32A,, Accessories for 3LD2 main control and EMERGENCYSTOP switches",9.32,"TEM",1,"LP",3.6999999999999998E-2,1]
["3LD92200C","neutral conductor, leading switching for floor mounting, up to 32A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",9.32,"TEM",1,"LP",3.5999999999999997E-2,1]
["3LD92202B","neutral conductor/PE terminal, throughtype, for front mounting, up to 32A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",7.35,"TEM",1,"LP",3.4000000000000002E-2,1]
["3LD92202C","neutral conductor/PE terminal, throughtype, for floor mounting, up to 32A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",7.35,"TEM",1,"LP",3.4000000000000002E-2,1]
["3LD92210A","Terminal covers, 3pole, for 25A and 32A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",3,"TEM",1,"LP",8.0000000000000002E-3,4]
["3LD92212A","Terminal covers, 1pole, for 25A and 32A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",74.31,"TEM",100,"LP",4.0000000000000001E-3,4]
["3LD92241B","rotary operating mechanism, selector switch black, for fourhole front mounting, for 25A and 32A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",4.8600000000000003,"TEM",1,"LP",7.5999999999999998E-2,1]
["3LD92241D","rotary operating mechanism, selector switch black, for centerhole front mounting, for 25A and 32A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",4.8600000000000003,"TEM",1,"LP",7.5999999999999998E-2,1]
["3LD92243B","rotary operating mechanism, selector switch red/yellow, for fourhole front mounting, for 25A and 32A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",4.8600000000000003,"TEM",1,"LP",7.5999999999999998E-2,1]
["3LD92243D","rotary operating mechanism, selector switch red/yellow, for centerhole front mounting, for 25A and 32A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",4.8600000000000003,"TEM",1,"LP",7.6999999999999999E-2,1]
["3LD92412A","Terminal covers, 1pole, for 160A and 250A, Accessories for 3LD23/24 main control and EMERGENCYSTOP switches",1.76,"TEM",1,"LP",1.8000000000000002E-2,4]
["3LD92500BA","neutral conductor, leading switching for front mounting, up to 63A,, Accessories for 3LD2 main control and EMERGENCYSTOP switches",14.9,"TEM",1,"LP",7.4999999999999997E-2,1]
["3LD92500CA","neutral conductor, leading switching for floor mounting, up to 63A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",14.9,"TEM",1,"LP",7.4999999999999997E-2,1]
["3LD92502BA","neutral conductor/PE terminal, throughtype, for front mounting, up to 63A, Accessories for 3LD25 main control and EMERGENCYSTOP switches",10.039999999999999,"TEM",1,"LP",6.7000000000000004E-2,1]
["3LD92502CA","neutral conductor/PE terminal, throughtype, for floor mounting, installation in distribution boards, molded plastic enclosure, up to 63A, Accessories for 3LD25 main control and EMERGENCYSTOP switches",10.039999999999999,"TEM",1,"LP",6.8000000000000005E-2,1]
["3LD92510A","Terminal covers, 3pole, for 63A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",3.31,"TEM",1,"LP",1.0999999999999999E-2,4]
["3LD92512A","Terminal covers, 1pole, for 63A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",101.53,"TEM",100,"LP",5.0000000000000001E-3,4]
["3LD92800B","neutral conductor, leading switching for front mounting, for 100A and 125A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",18.32,"TEM",1,"LP",9.6000000000000002E-2,1]
["3LD92800C","neutral conductor, leading switching for floor mounting, for 100A and 125A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",18.32,"TEM",1,"LP",9.7000000000000003E-2,1]
["3LD92802C","neutral conductor/PE terminal, throughtype, for floor mounting, for 100A and 125A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",12.32,"TEM",1,"LP",8.5999999999999993E-2,1]
["3LD92812A","Terminal covers, 1pole, for 100A and 125A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",1.24,"TEM",1,"LP",6.0000000000000001E-3,4]
["3LD92841B","rotary operating mechanism, selector switch black, for fourhole front mounting, for 63A and 125A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",12.94,"TEM",1,"LP",0.151,1]
["3LD92841D","rotary operating mechanism, selector switch black, for centerhole front mounting, for 63A, Accessories for 3LD2 main control and EMERGENCY STOP switches",12.94,"TEM",1,"LP",0.15,1]
["3LD92843B","rotary operating mechanism, selector switch red/yellow, for fourhole front mounting, for 63A to 125A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",12.94,"TEM",1,"LP",0.152,1]
["3LD92861A","additional label, German/English, 47mmx17mm, Accessories for 3LD2 main control and EMERGENCYSTOP switches",2.17,"TEM",1,"LP",5.1999999999999998E-2,10]
["3LD20640TB53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:16 A, Operational power / at AC23 A at 400 V: 7,5 kW, molded plastic enclosure for metric threaded joint, rotary operating mechanism, red/yellow",33.020000000000003,"TEM",1,"LP",0.46800000000000003,1]
["3LD22130TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, floor mounting with door coupling, rotary operating mechanism, black, 4 hole mounting of the handle",44.61,"TEM",1,"LP",0.40899999999999997,1]
["3LD23180TK11","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:160 A, Operational power / at AC23 A at 400 V: 75 kW, floor mounting with door coupling, knoboperated mechanism, black, 4hole mounting of the handle",263.2,"TEM",1,"LP",2.75,1]
["3LD25140TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, floor mounting with door coupling, rotary operating mechanism, black, 4 hole mounting of the handle",53.51,"TEM",1,"LP",0.63800000000000001,1]
["3LD28140TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:125 A, Operational power / at AC23 A at 400 V: 45 kW, floor mounting with door coupling, rotary operating mechanism, black, 4 hole mounting of the handle",109.71,"TEM",1,"LP",0.752,1]
["3LD92052C","shaft set, for rotary operating mechanism shaft 6x6mm, length 600mm, Accessories for 3LD2 main control and EMERGENCYSTOP switches",12.52,"TEM",1,"LP",0.84299999999999997,5]
["3LD92841B","rotary operating mechanism, selector switch black, for fourhole front mounting, for 63A and 125A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",12.94,"TEM",1,"LP",0.151,1]
["3LD20030TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:16 A, Operational power / at AC23 A at 400 V: 7,5 kW, frontmounted, rotary operating mechanism, black, 4 hole mounting of the handle",22.67,"TEM",1,"LP",0.20799999999999999,1]
["3LD20030TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:16 A, Operational power / at AC23 A at 400 V: 7,5 kW, front mounted, rotary operating mechanism, red/yellow, 4hole mounting of the handle",22.67,"TEM",1,"LP",0.20599999999999999,1]
["3LD20031TL51","SENTRON, 3LD switch disconnector, main switch, 4 pole, Iu:16 A, Operational power / at AC23 A at 400 V: 7,5 kW, frontmounted, rotary operating mechanism, black, 4 hole mounting of the handle",28.67,"TEM",1,"LP",0.218,1]
["3LD20031TL53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 4pole, Iu:16 A, Operational power / at AC23 A at 400 V: 7,5 kW, front mounted, rotary operating mechanism, red/yellow, 4hole mounting of the handle",28.67,"TEM",1,"LP",0.22,1]
["3LD20031TP53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:16 A, Operational power / at AC23 A at 400 V: 7,5 kW, front mounted, 1NC, 1NO, rotary operating mechanism, red/yellow, 4hole mounting of the handle",28.98,"TEM",1,"LP",0.22900000000000001,1]
["3LD20130TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:16 A, Operational power / at AC23 A at 400 V: 7,5 kW, floor mounting with door coupling, rotary operating mechanism, black, 4 hole mounting of the handle",36.54,"TEM",1,"LP",0.41299999999999998,1]
["3LD20130TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:16 A, Operational power / at AC23 A at 400 V: 7,5 kW, floor mounting with door coupling, rotary operating mechanism, red/yellow, 4hole mounting of the handle",36.54,"TEM",1,"LP",0.41,1]
["3LD20131TL51","SENTRON, 3LD switch disconnector, main switch, 4 pole, Iu:16 A, Operational power / at AC23 A at 400 V: 7,5 kW, floor mounting with door coupling, rotary operating mechanism, black, 4 hole mounting of the handle",41.61,"TEM",1,"LP",0.42,1]
["3LD20220TK11","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:16 A, Operational power / at AC23 A at 400 V: 7,5 kW, frontmounted, knob operated mechanism, black, 4 hole mounting of the handle",20.39,"TEM",1,"LP",0.184,1]
["3LD20220TK13","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:16 A, Operational power / at AC23 A at 400 V: 7,5 kW, front mounted, knoboperated mechanism, red/yellow, 4hole mounting of the handle",20.39,"TEM",1,"LP",0.183,1]
["3LD20300TK11","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:16 A, Operational power / at AC23 A at 400 V: 7,5 kW, Distribution board mounting, knoboperated mechanism, black, handle directly on switch",19.87,"TEM",1,"LP",0.16900000000000001,1]
["3LD20301TL11","SENTRON, 3LD switch disconnector, main switch, 4 pole, Iu:16 A, Operational power / at AC23 A at 400 V: 7,5 kW, Distribution board mounting, knoboperated mechanism, black, handle directly on switch",25.15,"TEM",1,"LP",0.183,1]
["3LD20440TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:16 A, Operational power / at AC23 A at 400 V: 7,5 kW, floor mounting with door coupling, rotary operating mechanism, red/yellow, center mounting 22.5 mm of handle",38.090000000000003,"TEM",1,"LP",0.437,1]
["3LD20500TK13","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:16 A, Operational power / at AC23 A at 400 V: 7,5 kW, front mounted, knoboperated mechanism, red/yellow, center mounting 22.5 mm of handle",22.25,"TEM",1,"LP",0.188,1]
["3LD20501TL11","SENTRON, 3LD switch disconnector, main switch, 4 pole, Iu:16 A, Operational power / at AC23 A at 400 V: 7,5 kW, frontmounted, knob operated mechanism, black, center mounting 22.5 mm of handle",28.46,"TEM",1,"LP",0.19800000000000001,1]
["3LD20540TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:16 A, Operational power / at AC23 A at 400 V: 7,5 kW, front mounted, rotary operating mechanism, red/yellow, center mounting 22.5 mm of handle",22.67,"TEM",1,"LP",0.20899999999999999,1]
["3LD20541TL53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 4pole, Iu:16 A, Operational power / at AC23 A at 400 V: 7,5 kW, front mounted, rotary operating mechanism, red/yellow, center mounting 22.5 mm of handle",29.29,"TEM",1,"LP",0.22,1]
["3LD20541TP51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:16 A, Operational power / at AC23 A at 400 V: 7,5 kW, frontmounted, 1NC, 1NO, rotary operating mechanism, black, center mounting 22.5 mm of handle",28.98,"TEM",1,"LP",0.23100000000000001,1]
["3LD20640TB51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:16 A, Operational power / at AC23 A at 400 V: 7,5 kW, moldedplastic enclosure for metric threaded joint, rotary operating mechanism, black",33.020000000000003,"TEM",1,"LP",0.46500000000000002,1]
["3LD20640TB53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:16 A, Operational power / at AC23 A at 400 V: 7,5 kW, molded plastic enclosure for metric threaded joint, rotary operating mechanism, red/yellow",33.020000000000003,"TEM",1,"LP",0.46800000000000003,1]
["3LD20641GP51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:16 A, Operational power / at AC23 A at 400 V: 7,5 kW, moldedplastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, black",41.5,"TEM",1,"LP",0.47699999999999998,1]
["3LD20641GP53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:16 A, Operational power / at AC23 A at 400 V: 7,5 kW, molded plastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, red/yellow",41.5,"TEM",1,"LP",0.47799999999999998,1]
["3LD20641TC53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 4pole, Iu:16 A, Operational power / at AC23 A at 400 V: 7,5 kW, molded plastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, red/yellow",48.23,"TEM",1,"LP",0.46899999999999997,1]
["3LD21030TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, frontmounted, rotary operating mechanism, black, 4 hole mounting of the handle",25.05,"TEM",1,"LP",0.20200000000000001,1]
["3LD21030TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, front mounted, rotary operating mechanism, red/yellow, 4hole mounting of the handle",25.05,"TEM",1,"LP",0.2,1]
["3LD21031TL53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 4pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, front mounted, rotary operating mechanism, red/yellow, 4hole mounting of the handle",31.36,"TEM",1,"LP",0.23500000000000001,1]
["3LD21031TP53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, front mounted, 1NC, 1NO, rotary operating mechanism, red/yellow, 4hole mounting of the handle",32.4,"TEM",1,"LP",0.222,1]
["3LD21033VK51","SENTRON, 3LD switch disconnector, main switch, 6 pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, frontmounted, rotary operating mechanism, black, 4 hole mounting of the handle",44.82,"TEM",1,"LP",0.38,1]
["3LD21033VK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 6pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, front mounted, rotary operating mechanism, red/yellow, 4hole mounting of the handle",44.82,"TEM",1,"LP",0.379,1]
["3LD21130TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, floor mounting with door coupling, rotary operating mechanism, black, 4 hole mounting of the handle",40.47,"TEM",1,"LP",0.40300000000000002,1]
["3LD21130TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, floor mounting with door coupling, rotary operating mechanism, red/yellow, 4hole mounting of the handle",40.47,"TEM",1,"LP",0.40400000000000003,1]
["3LD21131TL51","SENTRON, 3LD switch disconnector, main switch, 4 pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, floor mounting with door coupling, rotary operating mechanism, black, 4 hole mounting of the handle",46.26,"TEM",1,"LP",0.439,1]
["3LD21133VK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 6pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, floor mounting with door coupling, rotary operating mechanism, red/yellow, 4hole mounting of the handle",59.62,"TEM",1,"LP",0.6,1]
["3LD21134VP53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 6pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, floor mounting with door coupling, 1NC, 1NO, rotary operating mechanism, red/yellow, 4hole mounting of the handle",65.62,"TEM",1,"LP",0.61099999999999999,1]
["3LD21220TK11","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, floor mounting with door coupling, knoboperated mechanism, black, 4hole mounting of the handle",22.25,"TEM",1,"LP",0.17699999999999999,1]
["3LD21237UK01","SENTRON, 3LD switch disconnector, Selector switch, 3pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, floor mounting with door coupling, knoboperated mechanism, black, 4hole mounting of the handle",49.78,"TEM",1,"LP",0.378,1]
["3LD21300TK11","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, Distribution board mounting, knoboperated mechanism, black, handle directly on switch",21.63,"TEM",1,"LP",0.16300000000000001,1]
["3LD21440TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, floor mounting with door coupling, rotary operating mechanism, red/yellow, center mounting 22.5 mm of handle",42.44,"TEM",1,"LP",0.41599999999999998,1]
["3LD21441TL51","SENTRON, 3LD switch disconnector, main switch, 4 pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, floor mounting with door coupling, rotary operating mechanism, black, center mounting 22.5 mm of handle",47.51,"TEM",1,"LP",0.46200000000000002,1]
["3LD21540TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, frontmounted, rotary operating mechanism, black, center mounting 22.5 mm of handle",25.05,"TEM",1,"LP",0.20200000000000001,1]
["3LD21540TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, front mounted, rotary operating mechanism, red/yellow, center mounting 22.5 mm of handle",25.05,"TEM",1,"LP",0.20400000000000001,1]
["3LD21541TL53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 4pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, front mounted, rotary operating mechanism, red/yellow, center mounting 22.5 mm of handle",31.36,"TEM",1,"LP",0.24399999999999999,1]
["3LD21541TP51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, frontmounted, 1NC, 1NO, rotary operating mechanism, black, center mounting 22.5 mm of handle",32.4,"TEM",1,"LP",0.22900000000000001,1]
["3LD21541TP53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, front mounted, 1NC, 1NO, rotary operating mechanism, red/yellow, center mounting 22.5 mm of handle",32.4,"TEM",1,"LP",0.22900000000000001,1]
["3LD21640TB51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, moldedplastic enclosure for metric threaded joint, rotary operating mechanism, black",36.020000000000003,"TEM",1,"LP",0.46,1]
["3LD21640TB53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, molded plastic enclosure for metric threaded joint, rotary operating mechanism, red/yellow",36.020000000000003,"TEM",1,"LP",0.45900000000000002,1]
["3LD21641GP51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, moldedplastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, black",46.06,"TEM",1,"LP",0.46700000000000003,1]
["3LD21641GP53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, molded plastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, red/yellow",46.06,"TEM",1,"LP",0.47,1]
["3LD21641TC53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 4pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, molded plastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, red/yellow",53.3,"TEM",1,"LP",0.48199999999999998,1]
["3LD21653VB51","SENTRON, 3LD switch disconnector, main switch, 6 pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, moldedplastic enclosure for metric threaded joint, rotary operating mechanism, black",63.03,"TEM",1,"LP",0.86799999999999999,1]
["3LD21653VB53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 6pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, molded plastic enclosure for metric threaded joint, rotary operating mechanism, red/yellow",63.03,"TEM",1,"LP",0.86599999999999999,1]
["3LD21654VD51","SENTRON, 3LD switch disconnector, main switch, 6 pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, moldedplastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, black",70.900000000000006,"TEM",1,"LP",0.877,1]
["3LD21654VD53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 6pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, molded plastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, red/yellow",70.900000000000006,"TEM",1,"LP",0.88200000000000001,1]
["3LD21657UB01","SENTRON, 3LD switch disconnector, Selector switch, 3pole, Iu:25 A, Operational power / at AC23 A at 400 V: 9,5 kW, moldedplastic enclosure for metric threaded joint, knoboperated mechanism, black",74.209999999999994,"TEM",1,"LP",0.89400000000000002,1]
["3LD22030TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, frontmounted, rotary operating mechanism, black, 4 hole mounting of the handle",27.95,"TEM",1,"LP",0.2,1]
["3LD22030TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, front mounted, rotary operating mechanism, red/yellow, 4hole mounting of the handle",27.95,"TEM",1,"LP",0.20100000000000001,1]
["3LD22031TL51","SENTRON, 3LD switch disconnector, main switch, 4 pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, frontmounted, rotary operating mechanism, black, 4 hole mounting of the handle",37.979999999999997,"TEM",1,"LP",0.23500000000000001,1]
["3LD22031TL53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 4pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, front mounted, rotary operating mechanism, red/yellow, 4hole mounting of the handle",37.979999999999997,"TEM",1,"LP",0.23400000000000001,1]
["3LD22031TP51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, frontmounted, 1NC, 1NO, rotary operating mechanism, black, 4hole mounting of the handle",38.5,"TEM",1,"LP",0.22,1]
["3LD22031TP53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, front mounted, 1NC, 1NO, rotary operating mechanism, red/yellow, 4hole mounting of the handle",38.5,"TEM",1,"LP",0.221,1]
["3LD22033VK51","SENTRON, 3LD switch disconnector, main switch, 6 pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, frontmounted, rotary operating mechanism, black, 4 hole mounting of the handle",50.4,"TEM",1,"LP",0.38,1]
["3LD22033VK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 6pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, front mounted, rotary operating mechanism, red/yellow, 4hole mounting of the handle",50.4,"TEM",1,"LP",0.38300000000000001,1]
["3LD22100TK000AB6","SENTRON, 3LD switch disconnector, Switch, 3pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, floor mounting with door coupling, without",34.78,"TEM",1,"LP",0.20300000000000001,1]
["3LD22130TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, floor mounting with door coupling, rotary operating mechanism, black, 4 hole mounting of the handle",44.61,"TEM",1,"LP",0.40899999999999997,1]
["3LD22130TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, floor mounting with door coupling, rotary operating mechanism, red/yellow, 4hole mounting of the handle",44.61,"TEM",1,"LP",0.40600000000000003,1]
["3LD22131TL53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 4pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, floor mounting with door coupling, rotary operating mechanism, red/yellow, 4hole mounting of the handle",50.82,"TEM",1,"LP",0.433,1]
["3LD22220TK11","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, frontmounted, knob operated mechanism, black, 4 hole mounting of the handle",26.91,"TEM",1,"LP",0.17599999999999999,1]
["3LD22220TK13","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, front mounted, knoboperated mechanism, red/yellow, 4hole mounting of the handle",26.91,"TEM",1,"LP",0.17799999999999999,1]
["3LD22237UK01","SENTRON, 3LD switch disconnector, Selector switch, 3pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, frontmounted, knob operated mechanism, black, 4 hole mounting of the handle",54.65,"TEM",1,"LP",0.375,1]
["3LD22237UL010AD8","SENTRON, 3LD switch disconnector, Selector switch, 4pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, frontmounted, knob operated mechanism, black, 4 hole mounting of the handle, can be locked in zero position",134.86000000000001,"TEM",1,"LP",0.73099999999999998,1]
["3LD22300TK11","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, Distribution board mounting, knoboperated mechanism, black, handle directly on switch",26.29,"TEM",1,"LP",0.161,1]
["3LD22300TK13","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, Distribution board mounting, knoboperated mechanism, red/yellow, handle directly on switch",26.29,"TEM",1,"LP",0.16200000000000001,1]
["3LD22440TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, floor mounting with door coupling, rotary operating mechanism, black, center mounting 22.5 mm of handle",47.71,"TEM",1,"LP",0.41399999999999998,1]
["3LD22440TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, floor mounting with door coupling, rotary operating mechanism, red/yellow, center mounting 22.5 mm of handle",47.71,"TEM",1,"LP",0.41399999999999998,1]
["3LD22540TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, frontmounted, rotary operating mechanism, black, center mounting 22.5 mm of handle",29.5,"TEM",1,"LP",0.20300000000000001,1]
["3LD22540TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, front mounted, rotary operating mechanism, red/yellow, center mounting 22.5 mm of handle",29.5,"TEM",1,"LP",0.20200000000000001,1]
["3LD22640TB51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, moldedplastic enclosure for metric threaded joint, rotary operating mechanism, black",42.54,"TEM",1,"LP",0.45300000000000001,1]
["3LD22640TB53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, molded plastic enclosure for metric threaded joint, rotary operating mechanism, red/yellow",42.54,"TEM",1,"LP",0.46100000000000002,1]
["3LD22641GP51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, moldedplastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, black",51.44,"TEM",1,"LP",0.47,1]
["3LD22641GP53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, molded plastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, red/yellow",51.44,"TEM",1,"LP",0.47099999999999997,1]
["3LD22641TC53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 4pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, molded plastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, red/yellow",60.03,"TEM",1,"LP",0.48599999999999999,1]
["3LD22653VB51","SENTRON, 3LD switch disconnector, main switch, 6 pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, moldedplastic enclosure for metric threaded joint, rotary operating mechanism, black",72.97,"TEM",1,"LP",0.86,1]
["3LD22653VB53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 6pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, molded plastic enclosure for metric threaded joint, rotary operating mechanism, red/yellow",72.97,"TEM",1,"LP",0.875,1]
["3LD22654VD53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 6pole, Iu:32 A, Operational power / at AC23 A at 400 V: 11,5 kW, molded plastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, red/yellow",82.08,"TEM",1,"LP",0.88400000000000001,1]
["3LD23050TK11","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:160 A, Operational power / at AC23 A at 400 V: 75 kW, frontmounted, knob operated mechanism, black, 4 hole mounting of the handle",238.88,"TEM",1,"LP",2.089,1]
["3LD23050TK13","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:160 A, Operational power / at AC23 A at 400 V: 75 kW, front mounted, knoboperated mechanism, red/yellow, 4hole mounting of the handle",238.88,"TEM",1,"LP",2.105,1]
["3LD23051TL13","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 4pole, Iu:160 A, Operational power / at AC23 A at 400 V: 75 kW, front mounted, knoboperated mechanism, red/yellow, 4hole mounting of the handle",291.66000000000003,"TEM",1,"LP",2.6030000000000002,1]
["3LD23053VK13","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 6pole, Iu:160 A, Operational power / at AC23 A at 400 V: 75 kW, front mounted, knoboperated mechanism, red/yellow, 4hole mounting of the handle",531.27,"TEM",1,"LP",3.9740000000000002,1]
["3LD23180TK11","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:160 A, Operational power / at AC23 A at 400 V: 75 kW, floor mounting with door coupling, knoboperated mechanism, black, 4hole mounting of the handle",263.2,"TEM",1,"LP",2.75,1]
["3LD23180TK13","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:160 A, Operational power / at AC23 A at 400 V: 75 kW, floor mounting with door coupling, knoboperated mechanism, red/yellow, 4hole mounting of the handle",263.2,"TEM",1,"LP",2.746,1]
["3LD23183VK13","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 6pole, Iu:160 A, Operational power / at AC23 A at 400 V: 75 kW, floor mounting with door coupling, knoboperated mechanism, red/yellow, 4hole mounting of the handle",561.38,"TEM",1,"LP",4.6639999999999997,1]
["3LD23300TK13","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:160 A, Operational power / at AC23 A at 400 V: 132 kW, Distribution board mounting, knoboperated mechanism, red/yellow, handle directly on switch",234.74,"TEM",1,"LP",2.048,1]
["3LD24050TK11","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:160 A, Operational power / at AC23 A at 400 V: 132 kW, frontmounted, knob operated mechanism, black, 4 hole mounting of the handle",289.18,"TEM",1,"LP",2.097,1]
["3LD24051TL13","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 4pole, Iu:160 A, Operational power / at AC23 A at 400 V: 132 kW, front mounted, knoboperated mechanism, red/yellow, 4hole mounting of the handle",347.66,"TEM",1,"LP",2.605,1]
["3LD24180TK11","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:250 A, Operational power / at AC23 A at 400 V: 132 kW, floor mounting with door coupling, knoboperated mechanism, black, 4hole mounting of the handle",318.47000000000003,"TEM",1,"LP",2.7610000000000001,1]
["3LD24183VK13","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 6pole, Iu:250 A, Operational power / at AC23 A at 400 V: 132 kW, floor mounting with door coupling, knoboperated mechanism, red/yellow, 4hole mounting of the handle",671.82,"TEM",1,"LP",4.5570000000000004,1]
["3LD24300TK13","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:250 A, Operational power / at AC23 A at 400 V: 132 kW, Distribution board mounting, knoboperated mechanism, red/yellow, handle directly on switch",286.8,"TEM",1,"LP",2.0470000000000002,1]
["3LD25040TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, frontmounted, rotary operating mechanism, black, 4 hole mounting of the handle",48.13,"TEM",1,"LP",0.41199999999999998,1]
["3LD25040TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, front mounted, rotary operating mechanism, red/yellow, 4hole mounting of the handle",48.13,"TEM",1,"LP",0.41299999999999998,1]
["3LD25041TL51","SENTRON, 3LD switch disconnector, main switch, 4 pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, frontmounted, rotary operating mechanism, black, 4 hole mounting of the handle",63.03,"TEM",1,"LP",0.48499999999999999,1]
["3LD25041TL53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 4pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, front mounted, rotary operating mechanism, red/yellow, 4hole mounting of the handle",63.03,"TEM",1,"LP",0.49,1]
["3LD25041TP53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, front mounted, 1NC, 1NO, rotary operating mechanism, red/yellow, 4hole mounting of the handle",58.68,"TEM",1,"LP",0.438,1]
["3LD25043VK51","SENTRON, 3LD switch disconnector, main switch, 6 pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, frontmounted, rotary operating mechanism, black, 4 hole mounting of the handle",74.62,"TEM",1,"LP",0.74399999999999999,1]
["3LD25140TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, floor mounting with door coupling, rotary operating mechanism, black, 4 hole mounting of the handle",53.51,"TEM",1,"LP",0.63800000000000001,1]
["3LD25140TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, floor mounting with door coupling, rotary operating mechanism, red/yellow, 4hole mounting of the handle",53.51,"TEM",1,"LP",0.64,1]
["3LD25141TL53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 4pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, floor mounting with door coupling, rotary operating mechanism, red/yellow, 4hole mounting of the handle",64.38,"TEM",1,"LP",0.71699999999999997,1]
["3LD25247UK01","SENTRON, 3LD switch disconnector, Selector switch, 3pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, frontmounted, knob operated mechanism, black, 4 hole mounting of the handle",90.15,"TEM",1,"LP",0.74,1]
["3LD25300TK11","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, Distribution board mounting, knoboperated mechanism, black, handle directly on switch",40.57,"TEM",1,"LP",0.30299999999999999,1]
["3LD25300TK13","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, Distribution board mounting, knoboperated mechanism, red/yellow, handle directly on switch",40.57,"TEM",1,"LP",0.29799999999999999,1]
["3LD25440TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, floor mounting with door coupling, rotary operating mechanism, red/yellow, center mounting 22.5 mm of handle",64.069999999999993,"TEM",1,"LP",0.59,1]
["3LD25450TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, floor mounting with door coupling, rotary operating mechanism, black, center mounting 22.5 mm of handle",64.069999999999993,"TEM",1,"LP",0.68899999999999995,1]
["3LD25450TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, floor mounting with door coupling, rotary operating mechanism, red/yellow, center mounting 22.5 mm of handle",64.069999999999993,"TEM",1,"LP",0.68500000000000005,1]
["3LD25550TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, frontmounted, rotary operating mechanism, black, center mounting 22.5 mm of handle",48.13,"TEM",1,"LP",0.41899999999999998,1]
["3LD25550TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, front mounted, rotary operating mechanism, red/yellow, center mounting 22.5 mm of handle",48.13,"TEM",1,"LP",0.41899999999999998,1]
["3LD25650TB51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, moldedplastic enclosure for metric threaded joint, rotary operating mechanism, black",70.790000000000006,"TEM",1,"LP",0.9,1]
["3LD25650TB53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, molded plastic enclosure for metric threaded joint, rotary operating mechanism, red/yellow",70.790000000000006,"TEM",1,"LP",0.90900000000000003,1]
["3LD25651GP51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, moldedplastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, black",80.010000000000005,"TEM",1,"LP",0.90700000000000003,1]
["3LD25651GP53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, molded plastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, red/yellow",80.010000000000005,"TEM",1,"LP",0.90100000000000002,1]
["3LD25651TC51","SENTRON, 3LD switch disconnector, main switch, 4 pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, moldedplastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, black",82.08,"TEM",1,"LP",0.95299999999999996,1]
["3LD25651TC53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 4pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, molded plastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, red/yellow",82.08,"TEM",1,"LP",0.95899999999999996,1]
["3LD25663VB51","SENTRON, 3LD switch disconnector, main switch, 6 pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, moldedplastic enclosure for metric threaded joint, rotary operating mechanism, black",151.11000000000001,"TEM",1,"LP",2.1360000000000001,1]
["3LD25663VB53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 6pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, molded plastic enclosure for metric threaded joint, rotary operating mechanism, red/yellow",151.11000000000001,"TEM",1,"LP",2.1280000000000001,1]
["3LD25664VD53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 6pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, molded plastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, red/yellow",151.11000000000001,"TEM",1,"LP",2.1379999999999999,1]
["3LD25667UB01","SENTRON, 3LD switch disconnector, Selector switch, 3pole, Iu:63 A, Operational power / at AC23 A at 400 V: 22 kW, moldedplastic enclosure for metric threaded joint, knoboperated mechanism, black",182.78,"TEM",1,"LP",2.1640000000000001,1]
["3LD27040TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, frontmounted, rotary operating mechanism, black, 4 hole mounting of the handle",73.069999999999993,"TEM",1,"LP",0.497,1]
["3LD27040TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, front mounted, rotary operating mechanism, red/yellow, 4hole mounting of the handle",73.069999999999993,"TEM",1,"LP",0.49399999999999999,1]
["3LD27041TP53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, front mounted, 1NC, 1NO, rotary operating mechanism, red/yellow, 4hole mounting of the handle",83.63,"TEM",1,"LP",0.51700000000000002,1]
["3LD27140TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, floor mounting with door coupling, rotary operating mechanism, black, 4 hole mounting of the handle",87.77,"TEM",1,"LP",0.755,1]
["3LD27140TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, floor mounting with door coupling, rotary operating mechanism, red/yellow, 4hole mounting of the handle",87.77,"TEM",1,"LP",0.755,1]
["3LD27247UK01","SENTRON, 3LD switch disconnector, Selector switch, 3pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, frontmounted, knob operated mechanism, black, 4 hole mounting of the handle",169.02,"TEM",1,"LP",0.95599999999999996,1]
["3LD27300TK11","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, Distribution board mounting, knoboperated mechanism, black, handle directly on switch",69.66,"TEM",1,"LP",0.375,1]
["3LD27300TK13","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, Distribution board mounting, knoboperated mechanism, red/yellow, handle directly on switch",69.66,"TEM",1,"LP",0.375,1]
["3LD27660TB51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, moldedplastic enclosure for metric threaded joint, rotary operating mechanism, black",160.84,"TEM",1,"LP",1.8859999999999999,1]
["3LD27660TB53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, molded plastic enclosure for metric threaded joint, rotary operating mechanism, red/yellow",160.84,"TEM",1,"LP",1.8939999999999999,1]
["3LD27661GP51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, moldedplastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, black",165.7,"TEM",1,"LP",1.8149999999999999,1]
["3LD27661GP53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, molded plastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, red/yellow",165.7,"TEM",1,"LP",1.8560000000000001,1]
["3LD27667UB01","SENTRON, 3LD switch disconnector, Selector switch, 3pole, Iu:100 A, Operational power / at AC23 A at 400 V: 37 kW, moldedplastic enclosure for metric threaded joint, knoboperated mechanism, black",300.56,"TEM",1,"LP",2.3090000000000002,1]
["3LD28040TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:125 A, Operational power / at AC23 A at 400 V: 45 kW, frontmounted, rotary operating mechanism, black, 4 hole mounting of the handle",92.63,"TEM",1,"LP",0.501,1]
["3LD28040TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:125 A, Operational power / at AC23 A at 400 V: 45 kW, front mounted, rotary operating mechanism, red/yellow, 4hole mounting of the handle",92.63,"TEM",1,"LP",0.496,1]
["3LD28041TP53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:125 A, Operational power / at AC23 A at 400 V: 45 kW, front mounted, 1NC, 1NO, rotary operating mechanism, red/yellow, 4hole mounting of the handle",103.19,"TEM",1,"LP",0.51500000000000001,1]
["3LD28140TK51","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:125 A, Operational power / at AC23 A at 400 V: 45 kW, floor mounting with door coupling, rotary operating mechanism, black, 4 hole mounting of the handle",109.71,"TEM",1,"LP",0.752,1]
["3LD28140TK53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:125 A, Operational power / at AC23 A at 400 V: 45 kW, floor mounting with door coupling, rotary operating mechanism, red/yellow, 4hole mounting of the handle",109.71,"TEM",1,"LP",0.754,1]
["3LD28300TK11","SENTRON, 3LD switch disconnector, main switch, 3 pole, Iu:125 A, Operational power / at AC23 A at 400 V: 45 kW, Distribution board mounting, knoboperated mechanism, black, handle directly on switch",89.32,"TEM",1,"LP",0.374,1]
["3LD28300TK13","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:125 A, Operational power / at AC23 A at 400 V: 45 kW, Distribution board mounting, knoboperated mechanism, red/yellow, handle directly on switch",89.32,"TEM",1,"LP",0.378,1]
["3LD28660TB53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:125 A, Operational power / at AC23 A at 400 V: 45 kW, molded plastic enclosure for metric threaded joint, rotary operating mechanism, red/yellow",291.66000000000003,"TEM",1,"LP",1.883,1]
["3LD28661GP53","SENTRON, 3LD switch disconnector, EMERGENCYSTOP switch, 3pole, Iu:125 A, Operational power / at AC23 A at 400 V: 45 kW, molded plastic enclosure for metric threaded joint, 1NC, 1NO, rotary operating mechanism, red/yellow",300.56,"TEM",1,"LP",1.819,1]
["3LD92002B","neutral conductor/PE terminal, throughtype, for front mounting, up to 16A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",6.93,"TEM",1,"LP",0.03,1]
["3LD92005B","Auxiliary switch, 1NO+1NC, lagging switching, Accessories for 3LD2 main control and EMERGENCYSTOP switches",10.66,"TEM",1,"LP",0.02,1]
["3LD92005C","Auxiliary switch, 1NO+1NC, Accessories for 3LD2 main control and EMERGENCYSTOP switches",10.66,"TEM",1,"LP",0.02,1]
["3LD92006C","Auxiliary switch, 2NO, Accessories for 3LD2 main control and EMERGENCYSTOP switches",11.9,"TEM",1,"LP",2.1000000000000001E-2,1]
["3LD92050C","shaft set, for rotary operating mechanism with door coupling, shaft 6x6mm, length 300 mm, Accessories for 3LD2 main control and EMERGENCY STOP switches",6.42,"TEM",1,"LP",0.47899999999999998,5]
["3LD92052C","shaft set, for rotary operating mechanism shaft 6x6mm, length 600mm, Accessories for 3LD2 main control and EMERGENCYSTOP switches",12.52,"TEM",1,"LP",0.84299999999999997,5]
["3LD92200B","neutral conductor, leading switching for front mounting, up to 32A,, Accessories for 3LD2 main control and EMERGENCYSTOP switches",9.32,"TEM",1,"LP",3.6999999999999998E-2,1]
["3LD92200C","neutral conductor, leading switching for floor mounting, up to 32A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",9.32,"TEM",1,"LP",3.5999999999999997E-2,1]
["3LD92202B","neutral conductor/PE terminal, throughtype, for front mounting, up to 32A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",7.35,"TEM",1,"LP",3.4000000000000002E-2,1]
["3LD92202C","neutral conductor/PE terminal, throughtype, for floor mounting, up to 32A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",7.35,"TEM",1,"LP",3.4000000000000002E-2,1]
["3LD92210A","Terminal covers, 3pole, for 25A and 32A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",3,"TEM",1,"LP",8.0000000000000002E-3,4]
["3LD92212A","Terminal covers, 1pole, for 25A and 32A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",74.31,"TEM",100,"LP",4.0000000000000001E-3,4]
["3LD92241B","rotary operating mechanism, selector switch black, for fourhole front mounting, for 25A and 32A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",4.8600000000000003,"TEM",1,"LP",7.5999999999999998E-2,1]
["3LD92241D","rotary operating mechanism, selector switch black, for centerhole front mounting, for 25A and 32A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",4.8600000000000003,"TEM",1,"LP",7.5999999999999998E-2,1]
["3LD92243B","rotary operating mechanism, selector switch red/yellow, for fourhole front mounting, for 25A and 32A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",4.8600000000000003,"TEM",1,"LP",7.5999999999999998E-2,1]
["3LD92243D","rotary operating mechanism, selector switch red/yellow, for centerhole front mounting, for 25A and 32A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",4.8600000000000003,"TEM",1,"LP",7.6999999999999999E-2,1]
["3LD92412A","Terminal covers, 1pole, for 160A and 250A, Accessories for 3LD23/24 main control and EMERGENCYSTOP switches",1.76,"TEM",1,"LP",1.8000000000000002E-2,4]
["3LD92500BA","neutral conductor, leading switching for front mounting, up to 63A,, Accessories for 3LD2 main control and EMERGENCYSTOP switches",14.9,"TEM",1,"LP",7.4999999999999997E-2,1]
["3LD92500CA","neutral conductor, leading switching for floor mounting, up to 63A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",14.9,"TEM",1,"LP",7.4999999999999997E-2,1]
["3LD92502BA","neutral conductor/PE terminal, throughtype, for front mounting, up to 63A, Accessories for 3LD25 main control and EMERGENCYSTOP switches",10.039999999999999,"TEM",1,"LP",6.7000000000000004E-2,1]
["3LD92502CA","neutral conductor/PE terminal, throughtype, for floor mounting, installation in distribution boards, molded plastic enclosure, up to 63A, Accessories for 3LD25 main control and EMERGENCYSTOP switches",10.039999999999999,"TEM",1,"LP",6.8000000000000005E-2,1]
["3LD92510A","Terminal covers, 3pole, for 63A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",3.31,"TEM",1,"LP",1.0999999999999999E-2,4]
["3LD92512A","Terminal covers, 1pole, for 63A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",101.53,"TEM",100,"LP",5.0000000000000001E-3,4]
["3LD92800B","neutral conductor, leading switching for front mounting, for 100A and 125A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",18.32,"TEM",1,"LP",9.6000000000000002E-2,1]
["3LD92800C","neutral conductor, leading switching for floor mounting, for 100A and 125A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",18.32,"TEM",1,"LP",9.7000000000000003E-2,1]
["3LD92802C","neutral conductor/PE terminal, throughtype, for floor mounting, for 100A and 125A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",12.32,"TEM",1,"LP",8.5999999999999993E-2,1]
["3LD92812A","Terminal covers, 1pole, for 100A and 125A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",1.24,"TEM",1,"LP",6.0000000000000001E-3,4]
["3LD92841B","rotary operating mechanism, selector switch black, for fourhole front mounting, for 63A and 125A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",12.94,"TEM",1,"LP",0.151,1]
["3LD92841D","rotary operating mechanism, selector switch black, for centerhole front mounting, for 63A, Accessories for 3LD2 main control and EMERGENCY STOP switches",12.94,"TEM",1,"LP",0.15,1]
["3LD92843B","rotary operating mechanism, selector switch red/yellow, for fourhole front mounting, for 63A to 125A, Accessories for 3LD2 main control and EMERGENCYSTOP switches",12.94,"TEM",1,"LP",0.152,1]
["3LD92861A","additional label, German/English, 47mmx17mm, Accessories for 3LD2 main control and EMERGENCYSTOP switches",2.17,"TEM",1,"LP",5.1999999999999998E-2,10]
["8US10114SL01","BUSBAR ADAPTER 40 MM BUSBAR SYSTEM FOR CIRCUITBREAKERS 3VL1 UP TO 160A WITH TERMINAL COVER WIDTH: 108 MM, LENGTH: 175 MM",110.85,"TEM",1,"LP",0.56399999999999995,1]
["8US10114TM00","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER 72MM WIDE 40MM SYSTEM, 5+10MM RAIL THICKNESS ADAPTER LENGTH 182 MM FOR ASSEMBLING WITH CIRCUIT BREAKER SIRIUS 3R MODULE S3 (100A) APPLIC. RANGE 480  690V",86.63,"TEM",1,"LP",0.45900000000000002,1]
["8US10505RK07","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER, 45MM WIDTH 40MM SYSTEM, 5+10MM RAILTHICK. OUTGOING TERM. TOP 1.5...4 MM2 WITH 1 SUPP. RAIL 35MM, ...25 A FOR ANY SURFACE MOUNTING, LENGTH 139 MM",31.67,"TEM",1,"LP",0.14599999999999999,1]
["8US10515DJ07","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER, WIDTH 45MM 40MM SYSTEM, 5+10MM RAIL STR. WITH 1 MOUNTING RAIL 35MM, UP TO 25A FOR CIRCUITBREAKER 3RV10, SIZE S00, S0, LENGTH 120MM,",20.8,"TEM",1,"LP",0.111,1]
["8US10515DK07","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER, WIDTH 45MM 40MM SYSTEM, 5+10MM RAIL STR. WITH 1 MOUNTING RAIL 35MM, UP TO 25A FOR SINGLE UNITS UP TO A WIDTH OF 45MM, LENGTH 139MM",30.95,"TEM",1,"LP",0.158,1]
["8US10605AK00","BUSBAR ADAPTER SYSTEM FEEDIN ADAPTER, 54MM WIDE 40MM SYSTEM, 5 + 10MM BUSBAR THICKNESS INCOMING CABLES AT BOTTOM 35MM2 (80A) OUTPUT ON TOP 16MM2 (32A) WITHOUT OUTPUT CABLE 1 SUPPORTING RAIL 35MM",50.3,"TEM",1,"LP",0.29199999999999998,1]
["8US10615DJ07","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER, WIDTH 55MM 40MM SYSTEM, 5+10MM RAIL STR. WITH 1 MOUNTING RAIL 35MM, UP TO 25A FOR CIRCUITBREAKER 3RV10 W. LATERAL AUXIL. CONTACT BLOCKS, LENGTH 120MM, SIZE S00, S0",21.11,"TEM",1,"LP",0.105,1]
["8US10615FK08","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER 54MM WIDE 40MM SYSTEM, 5+10MM BUSBAR THICKNESS WITH 1 SUPPORTING RAIL 35MM, UP TO 56A LENGTH 139MM",40.47,"TEM",1,"LP",0.21299999999999999,4]
["8US10615FP08","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER 54MM WIDE 60MM SYSTEM, 5+10MM BUSBAR THICKNESS WITH 1 SUPPORTING RAIL 35MM, UP TO 56A E.G. FOR LIMITER 3VU1938 WITH FEEDIN TERMINAL 3VU91351BB01",46.89,"TEM",1,"LP",0.308,1]
["8US11114SM00","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER, WIDTH 70MM F. CIRCUITBREAKER 40/60MM SYSTEM, FOR SINGLE UNITS OF MOTOR FEEDERS 3RV1, 3RT1, 3RA1 LENGTH 182MM NOTE: ONLY SUITABLE 400V/50KA OR UP TO 460V/25KA",75.56,"TEM",1,"LP",0.504,1]
["8US12104AF00","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER 185MM WIDE FOR SWITCHING UNITS UP TO 630A (3KA53,3KL52/53,3NP42, WITH 3VF4/5, 3VL14, IN CONNECTION WITH 8US19274AF0 MOUNTING PLATE ONLY. 60MM SYSTEM, 5 + 10MM BUSBAR THICKNESS WITHOUT CONNECTION WIRING",170.67,"TEM",1,"LP",2.6509999999999998,1]
["8US12104AG00","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER 250MM WIDE FOR SWITCHING UNITS UP TO 630A 3NP52/53) 60MM SYSTEM, 5 + 10MM BUSBAR THICKNESS WITHOUT CONNECTION WIRING",175.95,"TEM",1,"LP",2.8679999999999999,1]
["8US12111NS10","BUSBAR SYSTEM BUSBAR CENTERTOCENTER CLEARANCE 60 MM DEVICE ADAPTER, WIDTH: 45 MM BUSBAR THICKN.:5.10MM+TTPROF. WITH 1 MOUNTING RAIL 35MM FOR COMPACT STARTER 3RA6 LENGTH 200MM UE 690V,IE UP TO 32A,ATTENTION: IF RATED CURRENT >12A AND SHORTCIRCUIT CURRENT>25KA MAX. CONDUCTOR CROSSSECT.6MM2 AND OBSERVE MIN. CONDUCTOR LENGTH",65.930000000000007,"TEM",1,"LP",0.315,1]
["8US12114SL00","BUSBAR ADAPTER 60 MM BUSBAR SYSTEM FOR CIRCUITBREAKERS 3VL3 UP TO 250A WITH TERMINAL COVER WIDTH: 108 MM, LENGTH: 175 MM",153.49,"TEM",1,"LP",0.63600000000000001,1]
["8US12114SL01","BUSBAR ADAPTER 60 MM BUSBAR SYSTEM FOR CIRCUITBREAKERS 3VL1/2 UP TO 160A WITH TERMINAL COVER WIDTH: 108 MM, LENGTH: 175 MM",97.19,"TEM",1,"LP",0.57299999999999995,1]
["8US12114TM00","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER 72MM WIDE 60MM SYSTEM, 5+10MM RAIL WIDTH ADAPTER LENGTH 182MM FOR ASSEMBLING WITH CIRCUIT BREAKER SIRIUS 3R MODULE S3 (100A) APPLIC. RANGE 480  690V",78.14,"TEM",1,"LP",0.47599999999999998,1]
["8US12114TR00","BUSBAR ADAPTER SYSTEM UL508A/IE BUSBAR ADAPTER SYSTEM 60MM BUSBAR WIDTH: 5/10MM/TTPROFILE UL RATING 80A/600V APPLICABLE IN FEEDER CIRCUITS IEC RATING 100A/690V FOR SIRIUS 3R CIRCUIT BREAKERS FOR SIRIUS 3R SIZE S3 LEAD OUTLET BOTTOM ADAPTER LENGTH 200MM ADAPTER WIDTH 72MM",98.53,"TEM",1,"LP",0.65,1]
["8US12134AF00","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER 185MM WIDE FOR SWITCHING UNITS UP TO 630A (3KA53,3KL52/53,3NP42, WITH 3VF4/5, 3VL14, IN CONNECTION WITH 8US19274AF0 MOUNTING PLATE ONLY. 60MM SYSTEM, 5 + 10MM BUSBAR THICKNESS WITHOUT CONNECTION WIRING",543.69000000000005,"TEM",1,"LP",3.141,1]
["8US12505AM00","BUSBAR ADAPTER SYSTEM CENTERTOCENTER CLEARANCE 60 MM DEVICE HOLDER, WIDTH 45MM RAIL WIDTH: 5+10MM TT SHAPE WITH 1 MOUNTING RAIL 35MM, FOR LATERAL MOUNTING TO ADAPTER 8US12, LENGTH 182MM *** UL508A FEEDER CIRCUIT ***",25.98,"TEM",1,"LP",0.14000000000000001,1]
["8US12505AT10","DEVICE HOLDER,45X260MM LONG FOR 60MM BUSBAR SYSTEM POSITIONER ENCLOSED 2 CONNECTING ELEMENTS ENCLOSED MOUNTING RAIL SCREWED ON",21.11,"TEM",1,"LP",0.24399999999999999,1]
["8US12505RM07","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER, 45MM WIDTH 60MM SYSTEM, 5+10MM RAILTHICK. OUTGOING TERM. TOP 1.5...4 MM2 WITH 1 SUPP. RAIL 35MM, ...25 A FOR ANY SURFACE MOUNTING LENGTH 182MM",31.36,"TEM",1,"LP",0.158,1]
["8US12515CM47","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER FOR SWITCHGEAR/CONTROL GEAR WITH CAGE CLAMP CONNECTION CABLE 2.5 MM2, 12.5A, 170MM LONG, ADAPTER 45MM WIDE, 182MM LANG WITH 1 SUPPORTING RAIL 35MM FOR 60MM RAIL SYSTEM FOR 5 OR 10MM BUSBAR THICKNESS FOR SWITCHGEAR/CONTROL GEAR AND SIRIUS 3R SIZE S00 MOTOR FEEDER",31.36,"TEM",1,"LP",0.188,1]
["8US12515DM07","BUSBAR SYSTEM BUSBAR CENTERTOCENTER CLEARANCE 60 MM DEVICE ADAPTER, WIDTH: 45 MM BUSBAR THICKNESS 5.10MM+TT PROFILE FOR CIRCUITBREAKERS, CONTACTORS, OVERLOAD RELAYS, MOTOR FEEDERS S00, S0, LENGTH 182MM WITH 1 SUPPORTING RAIL 35 MM, UP TO 25 A",31.36,"TEM",1,"LP",0.16800000000000001,6]
["8US12515DS10","DEVICE ADAPTER S00/S0, 25A, FOR 60MM BUSBAR SYSTEM 45X200MM LONG SPECIAL CABLES WELDED ON, AWG 12, 99 MM POSITIONER ENCLOSED MOUNTING RAIL SCREWED ON",26.19,"TEM",1,"LP",0.308,1]
["8US12515NT10","DEVICE ADAPTER S0, 32A, FOR 60MM BUSBAR SYSTEM, 45X260MM LONG SPECIAL CABLES WELDED ON AWG 10, 99MM LONG WITH POSITIONER SUPPORT RAIL SCREWED ON",29.39,"TEM",1,"LP",0.33400000000000002,1]
["8US12605AM00","BUSBAR ADAPTER SYSTEM DEVICE HOLDER 55MM WIDE 60MM SYSTEM, 5 + 10MM BUSBAR THICKNESS FOR LATERAL FITTING ON TO ADAPTER 8US1261.NA00 WITH 2 SUPPORTING RAILS 35MM",29.5,"TEM",1,"LP",0.17799999999999999,1]
["8US12605AP00","BUSBAR ADAPTER SYSTEM DEVICE HOLDER SPACER AND SHEET METAL SCREW ENCLOSED, F. LATERAL MOUNTING ONTO ADAPTER 8US12 LENGTH 242MM",33.74,"TEM",1,"LP",0.215,1]
["8US12615FM08","BUSBAR ADAPTER SYSTEM DEVICE HOLDER, 60MM SYSTEM, WITH 1 MOUNTING RAIL 35MM, UP TO 56A FOR 1 CONTACTOR WITH OVERLOAD RELAY 3R SIZE S2, LENGTH 182MM",40.159999999999997,"TEM",1,"LP",0.23200000000000001,1]
["8US12615FP08","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER, WIDTH 55MM 60MM SYSTEM, 5+10MM RAIL STR. WITH 1 MOUNTING RAIL 35MM, UP TO 56A FOR 1 CIRCUITBREAKER WITH CONTACTOR 3R SIZE S2, LENGTH 242MM",44.61,"TEM",1,"LP",0.28499999999999998,1]
["8US19033AB00","BUSBAR HOLDER 40 MM SYSTEM 1 X 12 X 5 MM, 2 X 12 X 5 MM EN END AND INTERMEDIATE HOLDER CONSISTS OF 2 HOLDERS",25.67,"TEM",1,"LP",0.17599999999999999,1]
["8US19033AB01","BUSBAR SUPPORT 40 MM SYSTEM 1 X 12 X 5 MM, 2 X 12 X 5 MM ASEND AND INTERM. SUPPORT",3.83,"TEM",1,"LP",9.2460000000000004,250]
["8US19211AA00","BUSBAR ADAPTER SYSTEM CONNECTION TERMINAL PLATE WITH COVER,84MM WIDE 60MM SYSTEM, 5 + 10MM BUSBAR THICKNESS 3 X 35120MM, WITH COVER",43.88,"TEM",1,"LP",0.496,1]
["8US19211BA00","TERMINAL BOARD 3POLE WITH COVER FOR BUS BAR 12X5 MM30X10 MM AND DOUBLE TPROFILE",36.229999999999997,"TEM",1,"LP",0.41699999999999998,1]
["8US19212AA00","BUSBAR ADAPTER SYSTEM TERMINALS FOR 5MM BUSBAR THICKNESS 1,516MM2",116.96,"TEM",100,"LP",2.1000000000000001E-2,100]
["8US19212AB00","BUSBAR SYSTEM, ACCESSORY FOR 40 AND 60 MM SYSTEM ONLY FOR 5MM BUSBAR THICKNESS",152.15,"TEM",100,"LP",4.5999999999999999E-2,50]
["8US19212AC00","BUSBAR ADAPTER SYSTEM TERMINALS FOR 5MM BUSBAR THICKNESS 16120MM2",6,"TEM",1,"LP",0.106,50]
["8US19212BB00","BUSBAR ADAPTER SYSTEM TERMINALS FOR 10MM BUSBAR THICKNESS 1,535MM2",3.93,"TEM",1,"LP",4.8000000000000001E-2,50]
["8US19212BB01","BUSBAR SYSTEM, ACCESSORIES CENTERCENTER DISTANCE 40.60 MM TERMINAL RAIL THICKNESS: 10MM+TT PROFILE 435 SQMM",4.24,"TEM",1,"LP",4.8000000000000001E-2,15]
["8US19212BC00","BUSBAR ADAPTER SYSTEM TERMINALS FOR 10MM BUSBAR THICKNESS 16120MM2",6,"TEM",1,"LP",0.107,50]
["8US19221AB00","BUSBAR ADAPTER SYSTEM END COVER FOR BUSBAR ENDS, FOR BUSBAR HOLDER 8US1 923 4POLE CONSISTS OF 2 PIECES",10.87,"TEM",1,"LP",5.3999999999999999E-2,1]
["8US19221AC00","BUSBAR ADAPTER SYSTEM END COVER FOR BUSBAR ENDS ON HOLDER 8US1923 3POLE",4.8600000000000003,"TEM",1,"LP",0.02,10]
["8US19221GA00","BUSBAR ADAPTER SYSTEM COVER, 84MM WIDE 40 + 60MM SYSTEM FOR TERMINALS UP TO 3 X 120MM2",15.53,"TEM",1,"LP",0.154,10]
["8US19221GA02","BUSBAR ADAPTER SYSTEM COVER, 270MM WIDE FOR TERMINALS UP TO 300MM2",32.4,"TEM",1,"LP",0.64500000000000002,1]
["8US19221GC00","BUSBAR SYSTEM, ACCESSORY BUSBAR CENTERTOCENTER CLEARANCE 60 MM COVER FOR 8US19412AA03/04",60.96,"TEM",1,"LP",0.34699999999999998,1]
["8US19222AA00","BUSBAR ADAPTER SYSTEM COVER PROFILE, 1000MM LONG FOR BUSBARS UP TO 30MM WIDTH AND 5MM THICKNESS",17.489999999999998,"TEM",1,"LP",0.15,10]
["8US19222AA01","BUSBAR SYSTEM, ACCESSORIES CENTERTOCENTER DISTANCE 40 MM INLAY PART 5 MM FOR BUSBAR HOLDER 8US19033AB01 CAUTION: SPECIAL TYPE",74.52,"TEM",100,"LP",0.623,600]
["8US19222BA00","BUSBAR ADAPTER SYSTEM COVER PROFILE, 1000MM LONG FOR BUSBARS UP TO 30MM WIDTH AND 10MM THICKNESS",18.940000000000001,"TEM",1,"LP",0.17499999999999999,10]
["8US19222CA00","BUSBAR SYSTEM, ACCESSORIES CENTERCENTER DISTANCE 40.60 MM COVER PROFILE FOR BUSBAR LENGTH: 1000 MM RAIL THICKNESS: 5 MM",3.21,"TEM",1,"LP",6.0999999999999999E-2,10]
["8US19222DA00","BUSBAR SYSTEM, ACCESSORIES CENTERCENTER DISTANCE 60 MM COVER PROFILE, TT BUSBAR LENGTH: 1000 MM",26.81,"TEM",1,"LP",0.48199999999999998,5]
["8US19222EA00","HOLDER FOR UNUSED PANEL 32MM FOR BUSBAR SYSTEM 60MM SUITABLE FOR COVER FOR UNUSED PANEL",9.2100000000000009,"TEM",1,"LP",3.7999999999999999E-2,4]
["8US19222EB00","HOLDER FOR UNUSED PANEL 195X700X63MM FOR BUSBAR SYSTEM 60MM FOR INSTALLATION ON HOLDER FOR UNUSED PANEL",34.67,"TEM",1,"LP",0.74099999999999999,2]
["8US19232AA01","BUSBAR SYSTEM, ACCESSORIES CENTERCENTER DISTANCE 60 MM BUSBAR HOLDER 3POLE FOR RAILS 12X5(10)30X5(10) EXTERNAL MOUNTING",18.63,"TEM",1,"LP",0.161,10]
["8US19233AA01","BUSBAR SYSTEM, ACCESSORIES CENTERCENTER DISTANCE 60 MM BUSBAR HOLDER 3POLE FOR RAILS 12X5(10)30X5(10) EXTERNAL MOUNTING",15.63,"TEM",1,"LP",0.154,10]
["8US19233UA01","BUSBAR SYSTEM, ACCESSORY BUSABR DISTANCE 60 MM BUSBAR SUPPORT FOR 12X5(10)30X5(10) PROFILES INSIDE FIXING WITH INC. CLEARANCE DISTANCES WITH INC. CREEPAGE DISTANCES CREEPAGE DISTANCES ACC. TO UL508",31.36,"TEM",1,"LP",0.154,10]
["8US19234AA00","BUSBAR ADAPTER SYSTEM BUSBAR HOLDER, 20MM WIDE 60MM SYSTEM FOR 4 BUSBARS 12 X 5(10)30 X 5(10) INSIDE FIXING",22.56,"TEM",1,"LP",0.23300000000000001,10]
["8US19235AA00","BUSBAR SYSTEM, ACCESSORIES CENTERCENTER DISTANCE 60 MM BUSBAR HOLDER 3POLE FOR RAILS 12X5(10)30X5(10) EXTERNAL MOUNTING",12.63,"TEM",1,"LP",0.112,10]
["8US19274AF01","MOUNTING PLATE FOR 8US12104AF00 FOR CIRCUITBREAKERS 3VL4 AND 3VL1 WITH RESIDUAL CURRENT DETECTION UP TO 400A",98.12,"TEM",1,"LP",0.54800000000000004,1]
["8US19412AA01","BUSBAR ADAPTER SYSTEM TERMINAL 95300MM2 FOR 10MM BUSBAR THICKNESS T AND DOUBLETPROFILE",16.559999999999999,"TEM",1,"LP",0.307,6]
["8US19412AA02","BUSBAR ADAPTER SYSTEM TERMINAL 150300MM2 FOR BUSBARS 20 X 530 X 10MM AS WELL AS FOR T AND DOUBLETPROFILE",23.08,"TEM",1,"LP",0.40600000000000003,3]
["8US19412AA03","TERMINAL SET, 3POLE CIRCULAR CONDUCTORS 120300MM2 BUSBAR CENTERTOCENTER CLEARANCE 60 MM IEC/UL508A *** COVER 8US19221GC00 MUST BE ORDERED SEPARATELY ***",158.77000000000001,"TEM",1,"LP",1.56,1]
["8US19412AA04","TERMINAL SET, 3POLE FOR FLAT BARS UP TO 32X20MM BUSBAR CENTERTOCENTER CLEARANCE 60 MM UL508A *** COVER 8US19221GC00 MUST BE ORDERED SEPARATELY ***",138.9,"TEM",1,"LP",1.339,1]
["8US19433AA00","BUSBAR SUPPORT WITH END CAP FOR DOPPELTPROFIL 3POLE LIGHT GRAY CONSISTS OF 4 PIECES",61.17,"TEM",1,"LP",1.0840000000000001,1]
["8US19482AA00","BUSBAR ADAPTER SYSTEM BUSBAR, 2400MM LONG ECU TINPLATED DOUBLETPROFILE, 1600A",547.72,"TEM",1,"LP",15.6,1]
["8US19981AA00","BUSBAR ADAPTER SYSTEM PACKAGE OF 100 CONNECTION KEYS FOR CONNECTING ADAPTERS WITH DEVICE HOLDERS WITH RACKS",41.4,"TEM",100,"LP",1E-3,100]
["8US19981AA10","CONNECTING ELEMENT",0.62,"TEM",1,"LP",1E-3,50]
["8US19981BA00","BUSBAR ADAPTER SYSTEM PACKAGE OF 100 CONNECTION KEYS FOR CONNECTING ADAPTERS WITH DEVICE HOLDERS WITH RACKS",61.17,"TEM",100,"LP",1E-3,100]
["8US19981BA10","SPACER",0.72,"TEM",1,"LP",2E-3,50]
["8US19982BJ10","SIDE MODULE 9 MM WIDE, 200 MM LONG, 63 MM DEEP. CENTERTOCENTER SPACING 60 MM FOR BUSBAR ADAPTER BUSBAR SYSTEM, ACCESSORIES BASIC BODY HALOGENFREE",8.07,"TEM",1,"LP",2.1000000000000001E-2,10]
["8US19987CA15","BUSBAR ADAPTER SYSTEM VERTICAL BUSBAR RUN MOUNTING RAIL 35 MM, PLASTIC WITH RECESS FOR INSERT 8US19981DA00, 45 MM LONG, WITH FIXING SCREWS FOR SIRIUS 3R ADAPTER S. S00 A. S0",1.76,"TEM",1,"LP",9.0000000000000011E-3,10]
["8US19987CA16","BUSBAR ADAPTER SYSTEM VERTICAL BUSBAR RUN MOUNTING RAIL 35 MM, PLASTIC WITH RECESS FOR INSERT 8US19981DA00, 55 MM LONG, WITH FIXING SCREWS FOR SIRIUS 3R ADAPTER S. S00 A. S0",2.2799999999999998,"TEM",1,"LP",0.01,10]
["8US19987CB45","BUSBAR ADAPTER SYSTEM VERTICAL BUSBAR RUN MOUNTING RAIL 35 MM, PLASTIC WITH RECESS FOR INSERT 8US19981DA00, 45 MM LONG, WITH FIXING SCREWS FOR SIRIUS 3R ADAPTER S. S00 A. S0",2.17,"TEM",1,"LP",1.4999999999999999E-2,10]
["8WC5052","FLAT COPPER BAR 15 X 5MM APPROX. 2 METERS LONG TINNED",84.87,"TEM",1,"LP",1.3280000000000001,1]
["8WC5065","FLAT COPPER BAR 30 X 10MM APPROX. 2 METERS LONG TINNED",297.98,"TEM",1,"LP",5.3639999999999999,1]
["8WC5120","FLAT COPPER BAR 6 X 6MM APPROX. 2,4 METERS LONG PLAIN",44.51,"TEM",1,"LP",0.8,1]
["8WC5123","FLAT COPPER BAR 12 X 5MM APPROX. 2,4 METERS LONG PLAIN",53.82,"TEM",1,"LP",1.2869999999999999,1]
["8WC5128","FLAT COPPER BAR 20 X 10MM APPROX. 2,4 METERS LONG PLAIN",124.92,"TEM",1,"LP",4.12,1]
["8WC5134","FLAT COPPER BAR 30 X 10MM APPROX. 2,4 METERS LONG PLAIN",189.41,"TEM",1,"LP",6.5,1]
["8US10114SL01","BUSBAR ADAPTER 40 MM BUSBAR SYSTEM FOR CIRCUITBREAKERS 3VL1 UP TO 160A WITH TERMINAL COVER WIDTH: 108 MM, LENGTH: 175 MM",110.85,"TEM",1,"LP",0.56399999999999995,1]
["8US10114TM00","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER 72MM WIDE 40MM SYSTEM, 5+10MM RAIL THICKNESS ADAPTER LENGTH 182 MM FOR ASSEMBLING WITH CIRCUIT BREAKER SIRIUS 3R MODULE S3 (100A) APPLIC. RANGE 480  690V",86.63,"TEM",1,"LP",0.45900000000000002,1]
["8US10505RK07","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER, 45MM WIDTH 40MM SYSTEM, 5+10MM RAILTHICK. OUTGOING TERM. TOP 1.5...4 MM2 WITH 1 SUPP. RAIL 35MM, ...25 A FOR ANY SURFACE MOUNTING, LENGTH 139 MM",31.67,"TEM",1,"LP",0.14599999999999999,1]
["8US10515DJ07","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER, WIDTH 45MM 40MM SYSTEM, 5+10MM RAIL STR. WITH 1 MOUNTING RAIL 35MM, UP TO 25A FOR CIRCUITBREAKER 3RV10, SIZE S00, S0, LENGTH 120MM,",20.8,"TEM",1,"LP",0.111,1]
["8US10515DK07","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER, WIDTH 45MM 40MM SYSTEM, 5+10MM RAIL STR. WITH 1 MOUNTING RAIL 35MM, UP TO 25A FOR SINGLE UNITS UP TO A WIDTH OF 45MM, LENGTH 139MM",30.95,"TEM",1,"LP",0.158,1]
["8US10605AK00","BUSBAR ADAPTER SYSTEM FEEDIN ADAPTER, 54MM WIDE 40MM SYSTEM, 5 + 10MM BUSBAR THICKNESS INCOMING CABLES AT BOTTOM 35MM2 (80A) OUTPUT ON TOP 16MM2 (32A) WITHOUT OUTPUT CABLE 1 SUPPORTING RAIL 35MM",50.3,"TEM",1,"LP",0.29199999999999998,1]
["8US10615DJ07","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER, WIDTH 55MM 40MM SYSTEM, 5+10MM RAIL STR. WITH 1 MOUNTING RAIL 35MM, UP TO 25A FOR CIRCUITBREAKER 3RV10 W. LATERAL AUXIL. CONTACT BLOCKS, LENGTH 120MM, SIZE S00, S0",21.11,"TEM",1,"LP",0.105,1]
["8US10615FK08","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER 54MM WIDE 40MM SYSTEM, 5+10MM BUSBAR THICKNESS WITH 1 SUPPORTING RAIL 35MM, UP TO 56A LENGTH 139MM",40.47,"TEM",1,"LP",0.21299999999999999,4]
["8US10615FP08","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER 54MM WIDE 60MM SYSTEM, 5+10MM BUSBAR THICKNESS WITH 1 SUPPORTING RAIL 35MM, UP TO 56A E.G. FOR LIMITER 3VU1938 WITH FEEDIN TERMINAL 3VU91351BB01",46.89,"TEM",1,"LP",0.308,1]
["8US11114SM00","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER, WIDTH 70MM F. CIRCUITBREAKER 40/60MM SYSTEM, FOR SINGLE UNITS OF MOTOR FEEDERS 3RV1, 3RT1, 3RA1 LENGTH 182MM NOTE: ONLY SUITABLE 400V/50KA OR UP TO 460V/25KA",75.56,"TEM",1,"LP",0.504,1]
["8US12104AF00","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER 185MM WIDE FOR SWITCHING UNITS UP TO 630A (3KA53,3KL52/53,3NP42, WITH 3VF4/5, 3VL14, IN CONNECTION WITH 8US19274AF0 MOUNTING PLATE ONLY. 60MM SYSTEM, 5 + 10MM BUSBAR THICKNESS WITHOUT CONNECTION WIRING",170.67,"TEM",1,"LP",2.6509999999999998,1]
["8US12104AG00","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER 250MM WIDE FOR SWITCHING UNITS UP TO 630A 3NP52/53) 60MM SYSTEM, 5 + 10MM BUSBAR THICKNESS WITHOUT CONNECTION WIRING",175.95,"TEM",1,"LP",2.8679999999999999,1]
["8US12111NS10","BUSBAR SYSTEM BUSBAR CENTERTOCENTER CLEARANCE 60 MM DEVICE ADAPTER, WIDTH: 45 MM BUSBAR THICKN.:5.10MM+TTPROF. WITH 1 MOUNTING RAIL 35MM FOR COMPACT STARTER 3RA6 LENGTH 200MM UE 690V,IE UP TO 32A,ATTENTION: IF RATED CURRENT >12A AND SHORTCIRCUIT CURRENT>25KA MAX. CONDUCTOR CROSSSECT.6MM2 AND OBSERVE MIN. CONDUCTOR LENGTH",65.930000000000007,"TEM",1,"LP",0.315,1]
["8US12114SL00","BUSBAR ADAPTER 60 MM BUSBAR SYSTEM FOR CIRCUITBREAKERS 3VL3 UP TO 250A WITH TERMINAL COVER WIDTH: 108 MM, LENGTH: 175 MM",153.49,"TEM",1,"LP",0.63600000000000001,1]
["8US12114SL01","BUSBAR ADAPTER 60 MM BUSBAR SYSTEM FOR CIRCUITBREAKERS 3VL1/2 UP TO 160A WITH TERMINAL COVER WIDTH: 108 MM, LENGTH: 175 MM",97.19,"TEM",1,"LP",0.57299999999999995,1]
["8US12114TM00","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER 72MM WIDE 60MM SYSTEM, 5+10MM RAIL WIDTH ADAPTER LENGTH 182MM FOR ASSEMBLING WITH CIRCUIT BREAKER SIRIUS 3R MODULE S3 (100A) APPLIC. RANGE 480  690V",78.14,"TEM",1,"LP",0.47599999999999998,1]
["8US12114TR00","BUSBAR ADAPTER SYSTEM UL508A/IE BUSBAR ADAPTER SYSTEM 60MM BUSBAR WIDTH: 5/10MM/TTPROFILE UL RATING 80A/600V APPLICABLE IN FEEDER CIRCUITS IEC RATING 100A/690V FOR SIRIUS 3R CIRCUIT BREAKERS FOR SIRIUS 3R SIZE S3 LEAD OUTLET BOTTOM ADAPTER LENGTH 200MM ADAPTER WIDTH 72MM",98.53,"TEM",1,"LP",0.65,1]
["8US12134AF00","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER 185MM WIDE FOR SWITCHING UNITS UP TO 630A (3KA53,3KL52/53,3NP42, WITH 3VF4/5, 3VL14, IN CONNECTION WITH 8US19274AF0 MOUNTING PLATE ONLY. 60MM SYSTEM, 5 + 10MM BUSBAR THICKNESS WITHOUT CONNECTION WIRING",543.69000000000005,"TEM",1,"LP",3.141,1]
["8US12505AM00","BUSBAR ADAPTER SYSTEM CENTERTOCENTER CLEARANCE 60 MM DEVICE HOLDER, WIDTH 45MM RAIL WIDTH: 5+10MM TT SHAPE WITH 1 MOUNTING RAIL 35MM, FOR LATERAL MOUNTING TO ADAPTER 8US12, LENGTH 182MM *** UL508A FEEDER CIRCUIT ***",25.98,"TEM",1,"LP",0.14000000000000001,1]
["8US12505AT10","DEVICE HOLDER,45X260MM LONG FOR 60MM BUSBAR SYSTEM POSITIONER ENCLOSED 2 CONNECTING ELEMENTS ENCLOSED MOUNTING RAIL SCREWED ON",21.11,"TEM",1,"LP",0.24399999999999999,1]
["8US12505RM07","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER, 45MM WIDTH 60MM SYSTEM, 5+10MM RAILTHICK. OUTGOING TERM. TOP 1.5...4 MM2 WITH 1 SUPP. RAIL 35MM, ...25 A FOR ANY SURFACE MOUNTING LENGTH 182MM",31.36,"TEM",1,"LP",0.158,1]
["8US12515CM47","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER FOR SWITCHGEAR/CONTROL GEAR WITH CAGE CLAMP CONNECTION CABLE 2.5 MM2, 12.5A, 170MM LONG, ADAPTER 45MM WIDE, 182MM LANG WITH 1 SUPPORTING RAIL 35MM FOR 60MM RAIL SYSTEM FOR 5 OR 10MM BUSBAR THICKNESS FOR SWITCHGEAR/CONTROL GEAR AND SIRIUS 3R SIZE S00 MOTOR FEEDER",31.36,"TEM",1,"LP",0.188,1]
["8US12515DM07","BUSBAR SYSTEM BUSBAR CENTERTOCENTER CLEARANCE 60 MM DEVICE ADAPTER, WIDTH: 45 MM BUSBAR THICKNESS 5.10MM+TT PROFILE FOR CIRCUITBREAKERS, CONTACTORS, OVERLOAD RELAYS, MOTOR FEEDERS S00, S0, LENGTH 182MM WITH 1 SUPPORTING RAIL 35 MM, UP TO 25 A",31.36,"TEM",1,"LP",0.16800000000000001,6]
["8US12515DS10","DEVICE ADAPTER S00/S0, 25A, FOR 60MM BUSBAR SYSTEM 45X200MM LONG SPECIAL CABLES WELDED ON, AWG 12, 99 MM POSITIONER ENCLOSED MOUNTING RAIL SCREWED ON",26.19,"TEM",1,"LP",0.308,1]
["8US12515NT10","DEVICE ADAPTER S0, 32A, FOR 60MM BUSBAR SYSTEM, 45X260MM LONG SPECIAL CABLES WELDED ON AWG 10, 99MM LONG WITH POSITIONER SUPPORT RAIL SCREWED ON",29.39,"TEM",1,"LP",0.33400000000000002,1]
["8US12605AM00","BUSBAR ADAPTER SYSTEM DEVICE HOLDER 55MM WIDE 60MM SYSTEM, 5 + 10MM BUSBAR THICKNESS FOR LATERAL FITTING ON TO ADAPTER 8US1261.NA00 WITH 2 SUPPORTING RAILS 35MM",29.5,"TEM",1,"LP",0.17799999999999999,1]
["8US12605AP00","BUSBAR ADAPTER SYSTEM DEVICE HOLDER SPACER AND SHEET METAL SCREW ENCLOSED, F. LATERAL MOUNTING ONTO ADAPTER 8US12 LENGTH 242MM",33.74,"TEM",1,"LP",0.215,1]
["8US12615FM08","BUSBAR ADAPTER SYSTEM DEVICE HOLDER, 60MM SYSTEM, WITH 1 MOUNTING RAIL 35MM, UP TO 56A FOR 1 CONTACTOR WITH OVERLOAD RELAY 3R SIZE S2, LENGTH 182MM",40.159999999999997,"TEM",1,"LP",0.23200000000000001,1]
["8US12615FP08","BUSBAR ADAPTER SYSTEM BUSBAR ADAPTER, WIDTH 55MM 60MM SYSTEM, 5+10MM RAIL STR. WITH 1 MOUNTING RAIL 35MM, UP TO 56A FOR 1 CIRCUITBREAKER WITH CONTACTOR 3R SIZE S2, LENGTH 242MM",44.61,"TEM",1,"LP",0.28499999999999998,1]
["8US19033AB00","BUSBAR HOLDER 40 MM SYSTEM 1 X 12 X 5 MM, 2 X 12 X 5 MM EN END AND INTERMEDIATE HOLDER CONSISTS OF 2 HOLDERS",25.67,"TEM",1,"LP",0.17599999999999999,1]
["8US19033AB01","BUSBAR SUPPORT 40 MM SYSTEM 1 X 12 X 5 MM, 2 X 12 X 5 MM ASEND AND INTERM. SUPPORT",3.83,"TEM",1,"LP",9.2460000000000004,250]
["8US19211AA00","BUSBAR ADAPTER SYSTEM CONNECTION TERMINAL PLATE WITH COVER,84MM WIDE 60MM SYSTEM, 5 + 10MM BUSBAR THICKNESS 3 X 35120MM, WITH COVER",43.88,"TEM",1,"LP",0.496,1]
["8US19211BA00","TERMINAL BOARD 3POLE WITH COVER FOR BUS BAR 12X5 MM30X10 MM AND DOUBLE TPROFILE",36.229999999999997,"TEM",1,"LP",0.41699999999999998,1]
["8US19212AA00","BUSBAR ADAPTER SYSTEM TERMINALS FOR 5MM BUSBAR THICKNESS 1,516MM2",116.96,"TEM",100,"LP",2.1000000000000001E-2,100]
["8US19212AB00","BUSBAR SYSTEM, ACCESSORY FOR 40 AND 60 MM SYSTEM ONLY FOR 5MM BUSBAR THICKNESS",152.15,"TEM",100,"LP",4.5999999999999999E-2,50]
["8US19212AC00","BUSBAR ADAPTER SYSTEM TERMINALS FOR 5MM BUSBAR THICKNESS 16120MM2",6,"TEM",1,"LP",0.106,50]
["8US19212BB00","BUSBAR ADAPTER SYSTEM TERMINALS FOR 10MM BUSBAR THICKNESS 1,535MM2",3.93,"TEM",1,"LP",4.8000000000000001E-2,50]
["8US19212BB01","BUSBAR SYSTEM, ACCESSORIES CENTERCENTER DISTANCE 40.60 MM TERMINAL RAIL THICKNESS: 10MM+TT PROFILE 435 SQMM",4.24,"TEM",1,"LP",4.8000000000000001E-2,15]
["8US19212BC00","BUSBAR ADAPTER SYSTEM TERMINALS FOR 10MM BUSBAR THICKNESS 16120MM2",6,"TEM",1,"LP",0.107,50]
["8US19221AB00","BUSBAR ADAPTER SYSTEM END COVER FOR BUSBAR ENDS, FOR BUSBAR HOLDER 8US1 923 4POLE CONSISTS OF 2 PIECES",10.87,"TEM",1,"LP",5.3999999999999999E-2,1]
["8US19221AC00","BUSBAR ADAPTER SYSTEM END COVER FOR BUSBAR ENDS ON HOLDER 8US1923 3POLE",4.8600000000000003,"TEM",1,"LP",0.02,10]
["8US19221GA00","BUSBAR ADAPTER SYSTEM COVER, 84MM WIDE 40 + 60MM SYSTEM FOR TERMINALS UP TO 3 X 120MM2",15.53,"TEM",1,"LP",0.154,10]
["8US19221GA02","BUSBAR ADAPTER SYSTEM COVER, 270MM WIDE FOR TERMINALS UP TO 300MM2",32.4,"TEM",1,"LP",0.64500000000000002,1]
["8US19221GC00","BUSBAR SYSTEM, ACCESSORY BUSBAR CENTERTOCENTER CLEARANCE 60 MM COVER FOR 8US19412AA03/04",60.96,"TEM",1,"LP",0.34699999999999998,1]
["8US19222AA00","BUSBAR ADAPTER SYSTEM COVER PROFILE, 1000MM LONG FOR BUSBARS UP TO 30MM WIDTH AND 5MM THICKNESS",17.489999999999998,"TEM",1,"LP",0.15,10]
["8US19222AA01","BUSBAR SYSTEM, ACCESSORIES CENTERTOCENTER DISTANCE 40 MM INLAY PART 5 MM FOR BUSBAR HOLDER 8US19033AB01 CAUTION: SPECIAL TYPE",74.52,"TEM",100,"LP",0.623,600]
["8US19222BA00","BUSBAR ADAPTER SYSTEM COVER PROFILE, 1000MM LONG FOR BUSBARS UP TO 30MM WIDTH AND 10MM THICKNESS",18.940000000000001,"TEM",1,"LP",0.17499999999999999,10]
["8US19222CA00","BUSBAR SYSTEM, ACCESSORIES CENTERCENTER DISTANCE 40.60 MM COVER PROFILE FOR BUSBAR LENGTH: 1000 MM RAIL THICKNESS: 5 MM",3.21,"TEM",1,"LP",6.0999999999999999E-2,10]
["8US19222DA00","BUSBAR SYSTEM, ACCESSORIES CENTERCENTER DISTANCE 60 MM COVER PROFILE, TT BUSBAR LENGTH: 1000 MM",26.81,"TEM",1,"LP",0.48199999999999998,5]
["8US19222EA00","HOLDER FOR UNUSED PANEL 32MM FOR BUSBAR SYSTEM 60MM SUITABLE FOR COVER FOR UNUSED PANEL",9.2100000000000009,"TEM",1,"LP",3.7999999999999999E-2,4]
["8US19222EB00","HOLDER FOR UNUSED PANEL 195X700X63MM FOR BUSBAR SYSTEM 60MM FOR INSTALLATION ON HOLDER FOR UNUSED PANEL",34.67,"TEM",1,"LP",0.74099999999999999,2]
["8US19232AA01","BUSBAR SYSTEM, ACCESSORIES CENTERCENTER DISTANCE 60 MM BUSBAR HOLDER 3POLE FOR RAILS 12X5(10)30X5(10) EXTERNAL MOUNTING",18.63,"TEM",1,"LP",0.161,10]
["8US19233AA01","BUSBAR SYSTEM, ACCESSORIES CENTERCENTER DISTANCE 60 MM BUSBAR HOLDER 3POLE FOR RAILS 12X5(10)30X5(10) EXTERNAL MOUNTING",15.63,"TEM",1,"LP",0.154,10]
["8US19233UA01","BUSBAR SYSTEM, ACCESSORY BUSABR DISTANCE 60 MM BUSBAR SUPPORT FOR 12X5(10)30X5(10) PROFILES INSIDE FIXING WITH INC. CLEARANCE DISTANCES WITH INC. CREEPAGE DISTANCES CREEPAGE DISTANCES ACC. TO UL508",31.36,"TEM",1,"LP",0.154,10]
["8US19234AA00","BUSBAR ADAPTER SYSTEM BUSBAR HOLDER, 20MM WIDE 60MM SYSTEM FOR 4 BUSBARS 12 X 5(10)30 X 5(10) INSIDE FIXING",22.56,"TEM",1,"LP",0.23300000000000001,10]
["8US19235AA00","BUSBAR SYSTEM, ACCESSORIES CENTERCENTER DISTANCE 60 MM BUSBAR HOLDER 3POLE FOR RAILS 12X5(10)30X5(10) EXTERNAL MOUNTING",12.63,"TEM",1,"LP",0.112,10]
["8US19274AF01","MOUNTING PLATE FOR 8US12104AF00 FOR CIRCUITBREAKERS 3VL4 AND 3VL1 WITH RESIDUAL CURRENT DETECTION UP TO 400A",98.12,"TEM",1,"LP",0.54800000000000004,1]
["8US19412AA01","BUSBAR ADAPTER SYSTEM TERMINAL 95300MM2 FOR 10MM BUSBAR THICKNESS T AND DOUBLETPROFILE",16.559999999999999,"TEM",1,"LP",0.307,6]
["8US19412AA02","BUSBAR ADAPTER SYSTEM TERMINAL 150300MM2 FOR BUSBARS 20 X 530 X 10MM AS WELL AS FOR T AND DOUBLETPROFILE",23.08,"TEM",1,"LP",0.40600000000000003,3]
["8US19412AA03","TERMINAL SET, 3POLE CIRCULAR CONDUCTORS 120300MM2 BUSBAR CENTERTOCENTER CLEARANCE 60 MM IEC/UL508A *** COVER 8US19221GC00 MUST BE ORDERED SEPARATELY ***",158.77000000000001,"TEM",1,"LP",1.56,1]
["8US19412AA04","TERMINAL SET, 3POLE FOR FLAT BARS UP TO 32X20MM BUSBAR CENTERTOCENTER CLEARANCE 60 MM UL508A *** COVER 8US19221GC00 MUST BE ORDERED SEPARATELY ***",138.9,"TEM",1,"LP",1.339,1]
["8US19433AA00","BUSBAR SUPPORT WITH END CAP FOR DOPPELTPROFIL 3POLE LIGHT GRAY CONSISTS OF 4 PIECES",61.17,"TEM",1,"LP",1.0840000000000001,1]
["8US19482AA00","BUSBAR ADAPTER SYSTEM BUSBAR, 2400MM LONG ECU TINPLATED DOUBLETPROFILE, 1600A",547.72,"TEM",1,"LP",15.6,1]
["8US19981AA00","BUSBAR ADAPTER SYSTEM PACKAGE OF 100 CONNECTION KEYS FOR CONNECTING ADAPTERS WITH DEVICE HOLDERS WITH RACKS",41.4,"TEM",100,"LP",1E-3,100]
["8US19981AA10","CONNECTING ELEMENT",0.62,"TEM",1,"LP",1E-3,50]
["8US19981BA00","BUSBAR ADAPTER SYSTEM PACKAGE OF 100 CONNECTION KEYS FOR CONNECTING ADAPTERS WITH DEVICE HOLDERS WITH RACKS",61.17,"TEM",100,"LP",1E-3,100]
["8US19981BA10","SPACER",0.72,"TEM",1,"LP",2E-3,50]
["8US19982BJ10","SIDE MODULE 9 MM WIDE, 200 MM LONG, 63 MM DEEP. CENTERTOCENTER SPACING 60 MM FOR BUSBAR ADAPTER BUSBAR SYSTEM, ACCESSORIES BASIC BODY HALOGENFREE",8.07,"TEM",1,"LP",2.1000000000000001E-2,10]
["8US19987CA15","BUSBAR ADAPTER SYSTEM VERTICAL BUSBAR RUN MOUNTING RAIL 35 MM, PLASTIC WITH RECESS FOR INSERT 8US19981DA00, 45 MM LONG, WITH FIXING SCREWS FOR SIRIUS 3R ADAPTER S. S00 A. S0",1.76,"TEM",1,"LP",9.0000000000000011E-3,10]
["8US19987CA16","BUSBAR ADAPTER SYSTEM VERTICAL BUSBAR RUN MOUNTING RAIL 35 MM, PLASTIC WITH RECESS FOR INSERT 8US19981DA00, 55 MM LONG, WITH FIXING SCREWS FOR SIRIUS 3R ADAPTER S. S00 A. S0",2.2799999999999998,"TEM",1,"LP",0.01,10]
["8US19987CB45","BUSBAR ADAPTER SYSTEM VERTICAL BUSBAR RUN MOUNTING RAIL 35 MM, PLASTIC WITH RECESS FOR INSERT 8US19981DA00, 45 MM LONG, WITH FIXING SCREWS FOR SIRIUS 3R ADAPTER S. S00 A. S0",2.17,"TEM",1,"LP",1.4999999999999999E-2,10]
["8WC5052","FLAT COPPER BAR 15 X 5MM APPROX. 2 METERS LONG TINNED",84.87,"TEM",1,"LP",1.3280000000000001,1]
["8WC5065","FLAT COPPER BAR 30 X 10MM APPROX. 2 METERS LONG TINNED",297.98,"TEM",1,"LP",5.3639999999999999,1]
["8WC5120","FLAT COPPER BAR 6 X 6MM APPROX. 2,4 METERS LONG PLAIN",44.51,"TEM",1,"LP",0.8,1]
["8WC5123","FLAT COPPER BAR 12 X 5MM APPROX. 2,4 METERS LONG PLAIN",53.82,"TEM",1,"LP",1.2869999999999999,1]
["8WC5128","FLAT COPPER BAR 20 X 10MM APPROX. 2,4 METERS LONG PLAIN",124.92,"TEM",1,"LP",4.12,1]
["8WC5134","FLAT COPPER BAR 30 X 10MM APPROX. 2,4 METERS LONG PLAIN",189.41,"TEM",1,"LP",6.5,1]
["8UD19002WB00","EXTENSION SHAFT 600MM, 8X8MM ACCESSORY FOR: DOOR COUPLING OPERATOR AND SIDE WALL MOUNTED OPERATOR 3VA",11.8,"TEM",1,"LP",0.28100000000000003,1]
["8UD19002WB00","EXTENSION SHAFT 600MM, 8X8MM ACCESSORY FOR: DOOR COUPLING OPERATOR AND SIDE WALL MOUNTED OPERATOR 3VA",11.8,"TEM",1,"LP",0.28100000000000003,1]
["4NC51120BC20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 3 50A/1A, 2,5VA PRIMARY CURRENT 50A, 2.5VA",62.31,"TEM",1,"LP",0.42399999999999999,1]
["4NC51122BC20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 3 50A/5A, 2,5VA PRIMARY CURRENT 50A, 2.5VA",57.44,"TEM",1,"LP",0.43,1]
["4NC51132BC20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 3 60A/5A, 2,5VA PRIMARY CURRENT 60A, 2.5VA",57.44,"TEM",1,"LP",0.42499999999999999,1]
["4NC51150BC20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 3 75A/1A, 2,5VA PRIMARY CURRENT 75A, 2.5VA",62.31,"TEM",1,"LP",0.42799999999999999,1]
["4NC51152BC20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 3 75A/5A, 2,5VA PRIMARY CURRENT 75A, 2.5VA",57.44,"TEM",1,"LP",0.42399999999999999,1]
["4NC51170CC20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 100A/1A, 2,5VA PRIMARY CURRENT 100A, 2.5VA",54.23,"TEM",1,"LP",0.33,1]
["4NC51172CC20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 100A/5A, 2,5VA PRIMARY CURRENT 100A, 2.5VA",48.96,"TEM",1,"LP",0.33600000000000002,1]
["4NC51210CC20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 150A/1A, 2,5VA PRIMARY CURRENT 150A, 2.5VA",54.23,"TEM",1,"LP",0.32,1]
["4NC51212CC20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 150A/5A, 2,5VA PRIMARY CURRENT 150A, 2.5VA",48.96,"TEM",1,"LP",0.32400000000000001,1]
["4NC51220CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 200A/1A, 5VA PRIMARY CURRENT 200A, 5VA",54.23,"TEM",1,"LP",0.35799999999999998,1]
["4NC51222CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 200A/5A, 5VA PRIMARY CURRENT 200A, 5VA",48.96,"TEM",1,"LP",0.34899999999999998,1]
["4NC51230CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 250A/1A, 5VA PRIMARY CURRENT 250A, 5VA",54.23,"TEM",1,"LP",0.34200000000000003,1]
["4NC51232CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 250A/5A, 5VA PRIMARY CURRENT 250A, 5VA",48.96,"TEM",1,"LP",0.34399999999999997,1]
["4NC52220CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 200A/1A, 5VA PRIMARY CURRENT 200A, 5VA",54.23,"TEM",1,"LP",0.45600000000000002,1]
["4NC52222CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 200A/5A, 5VA PRIMARY CURRENT 200A, 5VA",48.96,"TEM",1,"LP",0.46100000000000002,1]
["4NC52230CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 250A/1A, 5VA PRIMARY CURRENT 250A, 5VA",54.23,"TEM",1,"LP",0.46600000000000003,1]
["4NC52232CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 250A/5A, 5VA PRIMARY CURRENT 250A, 5VA",48.96,"TEM",1,"LP",0.46600000000000003,1]
["4NC52240CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 300A/1A, 5VA PRIMARY CURRENT 300A, 5VA",54.23,"TEM",1,"LP",0.35899999999999999,1]
["4NC52242CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 300A/5A, 5VA PRIMARY CURRENT 300A, 5VA",48.96,"TEM",1,"LP",0.35899999999999999,1]
["4NC52250CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 400A/1A, 5VA PRIMARY CURRENT 400A, 5VA",54.23,"TEM",1,"LP",0.371,1]
["4NC52252CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 400A/5A, 5VA PRIMARY CURRENT 400A, 5VA",48.96,"TEM",1,"LP",0.374,1]
["4NC53250CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 400A/1A, 5VA PRIMARY CURRENT 400A, 5VA",62.31,"TEM",1,"LP",0.46,1]
["4NC53252CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 400A/5A, 5VA PRIMARY CURRENT 400A, 5VA",57.44,"TEM",1,"LP",0.46100000000000002,1]
["4NC53260CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 500A/1A, 5VA PRIMARY CURRENT 500A, 5VA",62.31,"TEM",1,"LP",0.41699999999999998,1]
["4NC53262CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 500A/5A, 5VA PRIMARY CURRENT 500A, 5VA",57.44,"TEM",1,"LP",0.41499999999999998,1]
["4NC53270CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 600A/1A, 5VA PRIMARY CURRENT 600A, 5VA",62.31,"TEM",1,"LP",0.43,1]
["4NC53272CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 600A/5A, 5VA PRIMARY CURRENT 600A, 5VA",57.44,"TEM",1,"LP",0.435,1]
["4NC53280CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 750A/1A, 5VA PRIMARY CURRENT 750A, 5VA",62.31,"TEM",1,"LP",0.39,1]
["4NC53282CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 750A/5A, 5VA PRIMARY CURRENT 750A, 5VA",57.44,"TEM",1,"LP",0.38800000000000001,1]
["4NC54310CH20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 1000A/1A, 10VA PRIMARY CURRENT 1000A, 10VA",96.46,"TEM",1,"LP",0.66400000000000003,1]
["4NC54312CH20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 1000A/5A, 10VA PRIMARY CURRENT 1000A, 10VA",83.84,"TEM",1,"LP",0.65700000000000003,1]
["4NC54330CH20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 1250A/1A, 10VA PRIMARY CURRENT 1250A, 10VA",100.81,"TEM",1,"LP",0.68100000000000005,1]
["4NC54332CH20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 1250A/5A, 10VA PRIMARY CURRENT 1250A, 10VA",87.25,"TEM",1,"LP",0.65,1]
["4NC54340CH20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 1500A/1A, 10VA PRIMARY CURRENT 1500A, 10VA",104.74,"TEM",1,"LP",0.70199999999999996,1]
["4NC54342CH20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 1500A/5A, 10VA PRIMARY CURRENT 1500A, 10VA",89.73,"TEM",1,"LP",0.70499999999999996,1]
["4NC54332CH20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 1250A/5A, 10VA PRIMARY CURRENT 1250A, 10VA",87.25,"TEM",1,"LP",0.65,1]
["4NC51120BC20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 3 50A/1A, 2,5VA PRIMARY CURRENT 50A, 2.5VA",62.31,"TEM",1,"LP",0.42399999999999999,1]
["4NC51122BC20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 3 50A/5A, 2,5VA PRIMARY CURRENT 50A, 2.5VA",57.44,"TEM",1,"LP",0.43,1]
["4NC51132BC20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 3 60A/5A, 2,5VA PRIMARY CURRENT 60A, 2.5VA",57.44,"TEM",1,"LP",0.42499999999999999,1]
["4NC51150BC20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 3 75A/1A, 2,5VA PRIMARY CURRENT 75A, 2.5VA",62.31,"TEM",1,"LP",0.42799999999999999,1]
["4NC51152BC20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 3 75A/5A, 2,5VA PRIMARY CURRENT 75A, 2.5VA",57.44,"TEM",1,"LP",0.42399999999999999,1]
["4NC51170CC20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 100A/1A, 2,5VA PRIMARY CURRENT 100A, 2.5VA",54.23,"TEM",1,"LP",0.33,1]
["4NC51172CC20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 100A/5A, 2,5VA PRIMARY CURRENT 100A, 2.5VA",48.96,"TEM",1,"LP",0.33600000000000002,1]
["4NC51210CC20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 150A/1A, 2,5VA PRIMARY CURRENT 150A, 2.5VA",54.23,"TEM",1,"LP",0.32,1]
["4NC51212CC20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 150A/5A, 2,5VA PRIMARY CURRENT 150A, 2.5VA",48.96,"TEM",1,"LP",0.32400000000000001,1]
["4NC51220CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 200A/1A, 5VA PRIMARY CURRENT 200A, 5VA",54.23,"TEM",1,"LP",0.35799999999999998,1]
["4NC51222CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 200A/5A, 5VA PRIMARY CURRENT 200A, 5VA",48.96,"TEM",1,"LP",0.34899999999999998,1]
["4NC51230CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 250A/1A, 5VA PRIMARY CURRENT 250A, 5VA",54.23,"TEM",1,"LP",0.34200000000000003,1]
["4NC51232CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 250A/5A, 5VA PRIMARY CURRENT 250A, 5VA",48.96,"TEM",1,"LP",0.34399999999999997,1]
["4NC52220CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 200A/1A, 5VA PRIMARY CURRENT 200A, 5VA",54.23,"TEM",1,"LP",0.45600000000000002,1]
["4NC52222CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 200A/5A, 5VA PRIMARY CURRENT 200A, 5VA",48.96,"TEM",1,"LP",0.46100000000000002,1]
["4NC52230CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 250A/1A, 5VA PRIMARY CURRENT 250A, 5VA",54.23,"TEM",1,"LP",0.46600000000000003,1]
["4NC52232CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 250A/5A, 5VA PRIMARY CURRENT 250A, 5VA",48.96,"TEM",1,"LP",0.46600000000000003,1]
["4NC52240CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 300A/1A, 5VA PRIMARY CURRENT 300A, 5VA",54.23,"TEM",1,"LP",0.35899999999999999,1]
["4NC52242CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 300A/5A, 5VA PRIMARY CURRENT 300A, 5VA",48.96,"TEM",1,"LP",0.35899999999999999,1]
["4NC52250CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 400A/1A, 5VA PRIMARY CURRENT 400A, 5VA",54.23,"TEM",1,"LP",0.371,1]
["4NC52252CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 400A/5A, 5VA PRIMARY CURRENT 400A, 5VA",48.96,"TEM",1,"LP",0.374,1]
["4NC53250CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 400A/1A, 5VA PRIMARY CURRENT 400A, 5VA",62.31,"TEM",1,"LP",0.46,1]
["4NC53252CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 400A/5A, 5VA PRIMARY CURRENT 400A, 5VA",57.44,"TEM",1,"LP",0.46100000000000002,1]
["4NC53260CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 500A/1A, 5VA PRIMARY CURRENT 500A, 5VA",62.31,"TEM",1,"LP",0.41699999999999998,1]
["4NC53262CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 500A/5A, 5VA PRIMARY CURRENT 500A, 5VA",57.44,"TEM",1,"LP",0.41499999999999998,1]
["4NC53270CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 600A/1A, 5VA PRIMARY CURRENT 600A, 5VA",62.31,"TEM",1,"LP",0.43,1]
["4NC53272CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 600A/5A, 5VA PRIMARY CURRENT 600A, 5VA",57.44,"TEM",1,"LP",0.435,1]
["4NC53280CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 750A/1A, 5VA PRIMARY CURRENT 750A, 5VA",62.31,"TEM",1,"LP",0.39,1]
["4NC53282CE20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 750A/5A, 5VA PRIMARY CURRENT 750A, 5VA",57.44,"TEM",1,"LP",0.38800000000000001,1]
["4NC54310CH20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 1000A/1A, 10VA PRIMARY CURRENT 1000A, 10VA",96.46,"TEM",1,"LP",0.66400000000000003,1]
["4NC54312CH20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 1000A/5A, 10VA PRIMARY CURRENT 1000A, 10VA",83.84,"TEM",1,"LP",0.65700000000000003,1]
["4NC54330CH20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 1250A/1A, 10VA PRIMARY CURRENT 1250A, 10VA",100.81,"TEM",1,"LP",0.68100000000000005,1]
["4NC54332CH20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 1250A/5A, 10VA PRIMARY CURRENT 1250A, 10VA",87.25,"TEM",1,"LP",0.65,1]
["4NC54340CH20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 1500A/1A, 10VA PRIMARY CURRENT 1500A, 10VA",104.74,"TEM",1,"LP",0.70199999999999996,1]
["4NC54342CH20","WINDOWTYPE CURRENT TRANSFORMER, CLASS 1 1500A/5A, 10VA PRIMARY CURRENT 1500A, 10VA",89.73,"TEM",1,"LP",0.70499999999999996,1]

{"sheet":"Sheet1","index":1,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["PA","PMD Data available"]
[""]
["VF","Sales Release"]
[""]
["LF","Delivery Release"]
[""]
["AE","Phase Out Announce"]
[""]
["TS","Prod. Cancellation"]
[""]
["MH","Prod. Discont."]
[""]
["AK","End Prod.Lifecycl."]